{"text_format":"1","workbook":"xlsx","n_sheets":10,"sheets":["Elteq","ABTECH","ANAMET-M","ANAMET-S","BIMED","REIKU-B","REIKU-G","TECHNIK","TECHNIK SPECIAL - AKCIA","List"],"not_rendered":{"charts":0,"images":10,"macros":1,"external_links":0,"defined_names":10,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Elteq","index":0,"n_rows":14298,"n_cols":16384,"rows_kept":3,"cut":true,"hidden":false,"merged":[],"bounds":{"rows_first":1,"rows_last":1,"rows_between":1,"halvings":10}}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Option","Sheet name","Prod"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 30,5"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ABTECH"]

{"sheet":"ABTECH","index":1,"n_rows":137,"n_cols":7,"rows_kept":137,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["sheetname","Objednávací kód","Rozmery v mm D x Š x H ","Popis","Balenie","Cena za kus","Cena za kus po zľave"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ABTECH"},null,null,"Hliníkové skrine"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ABTECH"},"ZAG 1"," 50 x  45 x  30",{"$f":"B6","v":"ZAG 1"},"1ks",7.8224055281268683,{"$f":"F6*(1-Elteq!$F$4)","v":7.8224055281268683}]
["ABTECH","ZAG 2"," 58 x  64 x  34",{"$f":"B7","v":"ZAG 2"},"1ks",9.5455361005526811,{"$f":"F7*(1-Elteq!$F$4)","v":9.5455361005526811}]
["ABTECH","ZAG 3"," 98 x  64 x  34","ZAG 3","1ks",10.817009100029875,{"$f":"F8*(1-Elteq!$F$4)","v":10.817009100029875}]
["ABTECH","ZAG 4","150 x  64 x  36","ZAG 4","1ks",14.41508791646087,{"$f":"F9*(1-Elteq!$F$4)","v":14.41508791646087}]
["ABTECH","ZAG 5"," 75 x  80 x  57","ZAG 5","1ks",13.857157973406693,{"$f":"F10*(1-Elteq!$F$4)","v":13.857157973406693}]
["ABTECH","ZAG 6","125 x  80 x  57","ZAG 6","1ks",16.980806566152161,{"$f":"F11*(1-Elteq!$F$4)","v":16.980806566152161}]
["ABTECH","ZAG 7","175 x  80 x  57","ZAG 7","1ks",19.781842606791479,{"$f":"F12*(1-Elteq!$F$4)","v":19.781842606791479}]
["ABTECH","ZAG 8","250 x  80 x  54","ZAG 8","1ks",33.403683189250152,{"$f":"F13*(1-Elteq!$F$4)","v":33.403683189250152}]
["ABTECH","ZAG 9","122 x 120 x  80","ZAG 9","1ks",31.376917273665608,{"$f":"F14*(1-Elteq!$F$4)","v":31.376917273665608}]
["ABTECH","ZAG 9.9","122 x 120 x  90","ZAG 9.9","1ks",33.942635923356903,{"$f":"F15*(1-Elteq!$F$4)","v":33.942635923356903}]
["ABTECH","ZAG 10","220 x 120 x  80","ZAG 10","1ks",36.310991599995027,{"$f":"F16*(1-Elteq!$F$4)","v":36.310991599995027}]
["ABTECH","ZAG 10.9","220 x 120 x  90","ZAG 10.9","1ks",42.755651758539138,{"$f":"F17*(1-Elteq!$F$4)","v":42.755651758539138}]
["ABTECH","ZAG 11","160 x 160 x  90","ZAG 11","1ks",41.48417875906194,{"$f":"F18*(1-Elteq!$F$4)","v":41.48417875906194}]
["ABTECH","ZAG 12","260 x 160 x  90","ZAG 12","1ks",53.0982306348835,{"$f":"F19*(1-Elteq!$F$4)","v":53.0982306348835}]
["ABTECH","ZAG 13","360 x 160 x  90","ZAG 13","1ks",65.061463155337592,{"$f":"F20*(1-Elteq!$F$4)","v":65.061463155337592}]
["ABTECH","ZAG 14","560 x 160 x  90","ZAG 14","1ks",111.5366478675712,{"$f":"F21*(1-Elteq!$F$4)","v":111.5366478675712}]
["ABTECH","ZAG 15","200 x 230 x 110","ZAG 15","1ks",85.207668173919544,{"$f":"F22*(1-Elteq!$F$4)","v":85.207668173919544}]
["ABTECH","ZAG 16","330 x 230 x 110","ZAG 16","1ks",113.80632205768273,{"$f":"F23*(1-Elteq!$F$4)","v":113.80632205768273}]
["ABTECH","ZAG 17","330 x 230 x 180","ZAG 17","1ks",171.36419679521015,{"$f":"F24*(1-Elteq!$F$4)","v":171.36419679521015}]
["ABTECH","ZAG 18","400 x 230 x 110","ZAG 18","1ks",173.04557750795161,{"$f":"F25*(1-Elteq!$F$4)","v":173.04557750795161}]
["ABTECH","ZAG 18.3","400 x 310 x 110","ZAG 18.3","1ks",230.13281746358297,{"$f":"F26*(1-Elteq!$F$4)","v":230.13281746358297}]
["ABTECH","ZAG 19","420 x 240 x 210","ZAG 19","1ks",332.64770019755031,{"$f":"F27*(1-Elteq!$F$4)","v":332.64770019755031}]
["ABTECH","ZAG 20","600 x 230 x 110","ZAG 20","1ks",223.2782495917746,{"$f":"F28*(1-Elteq!$F$4)","v":223.2782495917746}]
["ABTECH","ZAG 21","360 x 120 x  80","ZAG 21","1ks",63.034697239753044,{"$f":"F29*(1-Elteq!$F$4)","v":63.034697239753044}]
["ABTECH","ZAG 22","280 x 230 x 110","ZAG 22","1ks",107.77156961240293,{"$f":"F30*(1-Elteq!$F$4)","v":107.77156961240293}]
["ABTECH",null,null,"Polyesterové skrine"]
["ABTECH","BPG 1"," 80 x  75 x  55",{"$f":"B32","v":"BPG 1"},"1ks",15.688432068740282,{"$f":"F32*(1-Elteq!$F$4)","v":15.688432068740282}]
["ABTECH","BPG 1.5"," 80 x  75 x  75",{"$f":"B33","v":"BPG 1.5"},"1ks",20.860442640852462,{"$f":"F33*(1-Elteq!$F$4)","v":20.860442640852462}]
["ABTECH","BPG 2","110 x  75 x  55","BPG 2","1ks",17.412435592777669,{"$f":"F34*(1-Elteq!$F$4)","v":17.412435592777669}]
["ABTECH","BPG 2.5","110 x  75 x  75","BPG 2.5","1ks",20.25704140743937,{"$f":"F35*(1-Elteq!$F$4)","v":20.25704140743937}]
["ABTECH","BPG 3","160 x  75 x  55","BPG 3","1ks",19.524339909723476,{"$f":"F36*(1-Elteq!$F$4)","v":19.524339909723476}]
["ABTECH","BPG 3.5","160 x  75 x  75","BPG 3.5","1ks",23.015447045899201,{"$f":"F37*(1-Elteq!$F$4)","v":23.015447045899201}]
["ABTECH","BPG 4","190 x  75 x  55","BPG 4","1ks",20.989742905155268,{"$f":"F38*(1-Elteq!$F$4)","v":20.989742905155268}]
["ABTECH","BPG 4.5","190 x  75 x  75","BPG 4.5","1ks",23.101647222101068,{"$f":"F39*(1-Elteq!$F$4)","v":23.101647222101068}]
["ABTECH","BPG 5","230 x  75 x  50","BPG 5","1ks",22.024145019577702,{"$f":"F40*(1-Elteq!$F$4)","v":22.024145019577702}]
["ABTECH","BPG 6","122 x 120 x  90","BPG 6","1ks",28.532258322818862,{"$f":"F41*(1-Elteq!$F$4)","v":28.532258322818862}]
["ABTECH","BPG 7","220 x 120 x  90","BPG 7","1ks",34.738671009353482,{"$f":"F42*(1-Elteq!$F$4)","v":34.738671009353482}]
["ABTECH","BPG 8","160 x 160 x  90","BPG 8","1ks",40.341682462475013,{"$f":"F43*(1-Elteq!$F$4)","v":40.341682462475013}]
["ABTECH","BPG 9","260 x 160 x  90","BPG 9","1ks",50.082302373286282,{"$f":"F44*(1-Elteq!$F$4)","v":50.082302373286282}]
["ABTECH","BPG 10","360 x 160 x  90","BPG 10","1ks",62.667528098759234,{"$f":"F45*(1-Elteq!$F$4)","v":62.667528098759234}]
["ABTECH","BPG 11","560 x 160 x  90","BPG 11","1ks",99.216402808351972,{"$f":"F46*(1-Elteq!$F$4)","v":99.216402808351972}]
["ABTECH","BPG 12","255 x 250 x 120","BPG 12","1ks",82.752169153794881,{"$f":"F47*(1-Elteq!$F$4)","v":82.752169153794881}]
["ABTECH","BPG 13","400 x 250 x 120","BPG 13","1ks",118.26664174896516,{"$f":"F48*(1-Elteq!$F$4)","v":118.26664174896516}]
["ABTECH","BPG 13.5","400 x 250 x 160","BPG 13.5","1ks",225.78835999999998,{"$f":"F49*(1-Elteq!$F$4)","v":225.78835999999998}]
["ABTECH","BPG 14","600 x 250 x 120","BPG 14","1ks",211.62143257559003,{"$f":"F50*(1-Elteq!$F$4)","v":211.62143257559003}]
["ABTECH","BPG 15","400 x 405 x 120","BPG 15","1ks",140.0752863280382,{"$f":"F51*(1-Elteq!$F$4)","v":140.0752863280382}]
["ABTECH",null,null,"Polycarbonátové skrine"]
["ABTECH","ZP 1"," 52 x  50 x  35",{"$f":"B53","v":"ZP 1"},"1ks",4.5255092505981569,{"$f":"F53*(1-Elteq!$F$4)","v":4.5255092505981569}]
["ABTECH","ZP 2"," 65 x  50 x  35",{"$f":"B54","v":"ZP 2"},"1ks",6.2926128627364841,{"$f":"F54*(1-Elteq!$F$4)","v":6.2926128627364841}]
["ABTECH","ZP 3"," 82 x  80 x  55","ZP 3","1ks",8.9217182368935077,{"$f":"F55*(1-Elteq!$F$4)","v":8.9217182368935077}]
["ABTECH","ZP 4"," 82 x  80 x  85","ZP 4","1ks",10.516421496628096,{"$f":"F56*(1-Elteq!$F$4)","v":10.516421496628096}]
["ABTECH","ZP 5","120 x  80 x  55","ZP 5","1ks",10.257820968022493,{"$f":"F57*(1-Elteq!$F$4)","v":10.257820968022493}]
["ABTECH","ZP 6","120 x  80 x  85","ZP 6","1ks",11.895624315858015,{"$f":"F58*(1-Elteq!$F$4)","v":11.895624315858015}]
["ABTECH","ZP 7","160 x  80 x  55","ZP 7","1ks",11.637023787252406,{"$f":"F59*(1-Elteq!$F$4)","v":11.637023787252406}]
["ABTECH","ZP 8","160 x  80 x  85","ZP 8","1ks",12.930026430280449,{"$f":"F60*(1-Elteq!$F$4)","v":12.930026430280449}]
["ABTECH","ZP 9","122 x 120 x  55","ZP 9","1ks",12.843826254078582,{"$f":"F61*(1-Elteq!$F$4)","v":12.843826254078582}]
["ABTECH","ZP 10","122 x 120 x  85","ZP 10","1ks",14.567829778115973,{"$f":"F62*(1-Elteq!$F$4)","v":14.567829778115973}]
["ABTECH","ZP 11","200 x 120 x  75","ZP 11","1ks",18.533037883401974,{"$f":"F63*(1-Elteq!$F$4)","v":18.533037883401974}]
["ABTECH","ZP 11.9 Shr","200 x 120 x  90","ZP 11.9 Shr","1ks",20.47254184794404,{"$f":"F64*(1-Elteq!$F$4)","v":20.47254184794404}]
["ABTECH","ZP 12","200 x 150 x  75","ZP 12","1ks",20.429441759843115,{"$f":"F65*(1-Elteq!$F$4)","v":20.429441759843115}]
["ABTECH","ZP 13","240 x 120 x 100","ZP 13","1ks",21.377643698063682,{"$f":"F66*(1-Elteq!$F$4)","v":21.377643698063682}]
["ABTECH","ZP 14","240 x 160 x  90","ZP 14","1ks",23.187847398302942,{"$f":"F67*(1-Elteq!$F$4)","v":23.187847398302942}]
["ABTECH","ZP 15","250 x 160 x  90","ZP 15","1ks",24.049849160321635,{"$f":"F68*(1-Elteq!$F$4)","v":24.049849160321635}]
["ABTECH","ZP 16","240 x 160 x 120","ZP 16","1ks",29.825260965846912,{"$f":"F69*(1-Elteq!$F$4)","v":29.825260965846912}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ABTECH"},"ZP 17","300 x 230 x  85","ZP 17","1ks",38.790079290841348,{"$f":"F70*(1-Elteq!$F$4)","v":38.790079290841348}]
["ABTECH","ZP 18","360 x 200 x 150","ZP 18","1ks",61.072824839024662,{"$f":"F71*(1-Elteq!$F$4)","v":61.072824839024662}]
["ABTECH","ZP 19","300 x 230 x 110","ZP 19","1ks",44.565491096366621,{"$f":"F72*(1-Elteq!$F$4)","v":44.565491096366621}]
["ABTECH","ZP 21 Shr"," 98 x  64 x  36","ZP 21 Shr","1ks",10.559521584729033,{"$f":"F73*(1-Elteq!$F$4)","v":10.559521584729033}]
["ABTECH","ZP 22 Shr","160 x 120 x  90","ZP 22 Shr","1ks",19.481239821622545,{"$f":"F74*(1-Elteq!$F$4)","v":19.481239821622545}]
["ABTECH","ZP 24 Shr","122 x 120 x 105","ZP 24 Shr","1ks",18.102037002392628,{"$f":"F75*(1-Elteq!$F$4)","v":18.102037002392628}]
["ABTECH","ZP 25 Shr","250 x 160 x 120","ZP 25 Shr","1ks",32.583666604306735,{"$f":"F76*(1-Elteq!$F$4)","v":32.583666604306735}]
["ABTECH","ZP 26 Shr","340 x 150 x 100","ZP 26 Shr","1ks",40.083081933869401,{"$f":"F77*(1-Elteq!$F$4)","v":40.083081933869401}]
["ABTECH",null,null,"ABS skrine"]
["ABTECH","ZPS 1"," 52 x  50 x  35",{"$f":"B79","v":"ZPS 1"},"1ks",3.7065579999999998,{"$f":"F79*(1-Elteq!$F$4)","v":3.7065579999999998}]
["ABTECH","ZPS 2"," 65 x  50 x  35",{"$f":"B80","v":"ZPS 2"},"1ks",5.3444109245159206,{"$f":"F80*(1-Elteq!$F$4)","v":5.3444109245159206}]
["ABTECH","ZPS 3"," 82 x  80 x  55","ZPS 3","1ks",7.3270149771589219,{"$f":"F81*(1-Elteq!$F$4)","v":7.3270149771589219}]
["ABTECH","ZPS 4"," 82 x  80 x  85","ZPS 4","1ks",8.5769175320860338,{"$f":"F82*(1-Elteq!$F$4)","v":8.5769175320860338}]
["ABTECH","ZPS 5","120 x  80 x  55","ZPS 5","1ks",8.4907173558841631,{"$f":"F83*(1-Elteq!$F$4)","v":8.4907173558841631}]
["ABTECH","ZPS 6","120 x  80 x  85","ZPS 6","1ks",9.611319646508468,{"$f":"F84*(1-Elteq!$F$4)","v":9.611319646508468}]
["ABTECH","ZPS 7","160 x  80 x  55","ZPS 7","1ks",9.697519822710337,{"$f":"F85*(1-Elteq!$F$4)","v":9.697519822710337}]
["ABTECH","ZPS 8","160 x  80 x  85","ZPS 8","1ks",10.645721760930904,{"$f":"F86*(1-Elteq!$F$4)","v":10.645721760930904}]
["ABTECH","ZPS 9","122 x 120 x  55","ZPS 9","1ks",10.171620791820622,{"$f":"F87*(1-Elteq!$F$4)","v":10.171620791820622}]
["ABTECH","ZPS 10","122 x 120 x  85","ZPS 10","1ks",11.809424139656144,{"$f":"F88*(1-Elteq!$F$4)","v":11.809424139656144}]
["ABTECH","ZPS 11","200 x 120 x  75","ZPS 11","1ks",14.654029954317844,{"$f":"F89*(1-Elteq!$F$4)","v":14.654029954317844}]
["ABTECH","ZPS 11.9 Shr","200 x 120 x  90","ZPS 11.9 Shr","1ks",17.153835064172068,{"$f":"F90*(1-Elteq!$F$4)","v":17.153835064172068}]
["ABTECH","ZPS 12","200 x 150 x  75","ZPS 12","1ks",17.498635768979547,{"$f":"F91*(1-Elteq!$F$4)","v":17.498635768979547}]
["ABTECH","ZPS 13","240 x 120 x 100","ZPS 13","1ks",18.188237178594505,{"$f":"F92*(1-Elteq!$F$4)","v":18.188237178594505}]
["ABTECH","ZPS 14","240 x 160 x  90","ZPS 14","1ks",18.619238059603845,{"$f":"F93*(1-Elteq!$F$4)","v":18.619238059603845}]
["ABTECH","ZPS 15","250 x 160 x  90","ZPS 15","1ks",19.739840350228157,{"$f":"F94*(1-Elteq!$F$4)","v":19.739840350228157}]
["ABTECH","ZPS 16","240 x 160 x 120","ZPS 16","1ks",24.394649865129111,{"$f":"F95*(1-Elteq!$F$4)","v":24.394649865129111}]
["ABTECH","ZPS 17","300 x 230 x  85","ZPS 17","1ks",34.652470833151604,{"$f":"F96*(1-Elteq!$F$4)","v":34.652470833151604}]
["ABTECH","ZPS 18","360 x 200 x 150","ZPS 18","1ks",42.841487572329221,{"$f":"F97*(1-Elteq!$F$4)","v":42.841487572329221}]
["ABTECH","ZPS 19","300 x 230 x 110","ZPS 19","1ks",39.134879995648831,{"$f":"F98*(1-Elteq!$F$4)","v":39.134879995648831}]
["ABTECH","ZPS 21 Shr"," 98 x  64  x  36","ZPS 21 Shr","1ks",7.1546146247551832,{"$f":"F99*(1-Elteq!$F$4)","v":7.1546146247551832}]
["ABTECH","ZPS 22 Shr","160 x 120 x  90","ZPS 22 Shr","1ks",17.671036121383285,{"$f":"F100*(1-Elteq!$F$4)","v":17.671036121383285}]
["ABTECH","ZPS 24 Shr","122 x 120 x 105","ZPS 24 Shr","1ks",15.688432068740282,{"$f":"F101*(1-Elteq!$F$4)","v":15.688432068740282}]
["ABTECH","ZPS 25 Shr","250 x 160 x 120","ZPS 25 Shr","1ks",28.359857970415121,{"$f":"F102*(1-Elteq!$F$4)","v":28.359857970415121}]
["ABTECH","ZPS 26 Shr","340 x 150 x 100","ZPS 26 Shr","1ks",35.255872066564699,{"$f":"F103*(1-Elteq!$F$4)","v":35.255872066564699}]
["ABTECH",null,null,"Hliníkové skrině EX"]
["ABTECH","ZAG-EX 2"," 58 x  64 x  34",{"$f":"B105","v":"ZAG-EX 2"},"1ks",16.938334623667387,{"$f":"F105*(1-Elteq!$F$4)","v":16.938334623667387}]
["ABTECH","ZAG-EX 3"," 98 x  64 x  34",{"$f":"B106","v":"ZAG-EX 3"},"1ks",18.274437354796373,{"$f":"F106*(1-Elteq!$F$4)","v":18.274437354796373}]
["ABTECH","ZAG-EX 4","150 x  64 x  36","ZAG-EX 4","1ks",21.248343433760873,{"$f":"F107*(1-Elteq!$F$4)","v":21.248343433760873}]
["ABTECH","ZAG-EX 5"," 75 x  80 x  57","ZAG-EX 5","1ks",20.300141495540309,{"$f":"F108*(1-Elteq!$F$4)","v":20.300141495540309}]
["ABTECH","ZAG-EX 6","125 x  80 x  57","ZAG-EX 6","1ks",24.049849160321635,{"$f":"F109*(1-Elteq!$F$4)","v":24.049849160321635}]
["ABTECH","ZAG-EX 7","175 x  80 x  57","ZAG-EX 7","1ks",26.463454093973986,{"$f":"F110*(1-Elteq!$F$4)","v":26.463454093973986}]
["ABTECH","ZAG-EX 9","122 x 120 x  80","ZAG-EX 9","1ks",42.755287396127365,{"$f":"F111*(1-Elteq!$F$4)","v":42.755287396127365}]
["ABTECH","ZAG-EX 9.9","122 x 120 x 90","ZAG-EX 9.9","1ks",62.154320000000006,{"$f":"F112*(1-Elteq!$F$4)","v":62.154320000000006}]
["ABTECH","ZAG-EX 10","220 x 120 x  80","ZAG-EX 10","1ks",47.884197880138601,{"$f":"F113*(1-Elteq!$F$4)","v":47.884197880138601}]
["ABTECH","ZAG-EX 10.9","220 x 120 x 90","ZAG-EX 10.9","1ks",69.599159999999998,{"$f":"F114*(1-Elteq!$F$4)","v":69.599159999999998}]
["ABTECH","ZAG-EX 11","160 x 160 x  90","ZAG-EX 11","1ks",50.64260351859842,{"$f":"F115*(1-Elteq!$F$4)","v":50.64260351859842}]
["ABTECH","ZAG-EX 12","260 x 160 x  90","ZAG-EX 12","1ks",58.142018848161101,{"$f":"F116*(1-Elteq!$F$4)","v":58.142018848161101}]
["ABTECH","ZAG-EX 13","360 x 160 x  90","ZAG-EX 13","1ks",70.253143604523785,{"$f":"F117*(1-Elteq!$F$4)","v":70.253143604523785}]
["ABTECH","ZAG-EX 15","200 x 230 x 110","ZAG-EX 15","1ks",81.545366686968677,{"$f":"F118*(1-Elteq!$F$4)","v":81.545366686968677}]
["ABTECH","ZAG-EX 16","330 x 230 x 110","ZAG-EX 16","1ks",113.69803241026609,{"$f":"F119*(1-Elteq!$F$4)","v":113.69803241026609}]
["ABTECH",null,null,"Polyesterové skrine EX"]
["ABTECH","BPG-EX 1"," 80 x  75 x  55",{"$f":"B121","v":"BPG-EX 1"},"1ks",23.963648984119768,{"$f":"F121*(1-Elteq!$F$4)","v":23.963648984119768}]
["ABTECH","BPG-EX 2","110 x  75 x  55",{"$f":"B122","v":"BPG-EX 2"},"1ks",25.860052860560899,{"$f":"F122*(1-Elteq!$F$4)","v":25.860052860560899}]
["ABTECH","BPG-EX 3","160 x  75 x  55","BPG-EX 3","1ks",27.97195717750671,{"$f":"F123*(1-Elteq!$F$4)","v":27.97195717750671}]
["ABTECH","BPG-EX 4","190 x  75 x  55","BPG-EX 4","1ks",29.652860613443167,{"$f":"F124*(1-Elteq!$F$4)","v":29.652860613443167}]
["ABTECH","BPG-EX 4.5","190 x  75 x  75","BPG-EX 4.5","1ks",30.342462023058122,{"$f":"F125*(1-Elteq!$F$4)","v":30.342462023058122}]
["ABTECH","BPG-EX 5","230 x  75 x  50","BPG-EX 5","1ks",30.730362815966537,{"$f":"F126*(1-Elteq!$F$4)","v":30.730362815966537}]
["ABTECH","BPG-EX 6","122 x 120 x  90","BPG-EX 6","1ks",38.014277705024519,{"$f":"F127*(1-Elteq!$F$4)","v":38.014277705024519}]
["ABTECH","BPG-EX 7","220 x 120 x  90","BPG-EX 7","1ks",44.565491096366621,{"$f":"F128*(1-Elteq!$F$4)","v":44.565491096366621}]
["ABTECH","BPG-EX 8","160 x 160 x  90","BPG-EX 8","1ks",50.858103959103104,{"$f":"F129*(1-Elteq!$F$4)","v":50.858103959103104}]
["ABTECH","BPG-EX 9","260 x 160 x  90","BPG-EX 9","1ks",82.66986,{"$f":"F130*(1-Elteq!$F$4)","v":82.66986}]
["ABTECH","BPG-EX 10","360 x 160 x  90","BPG-EX 10","1ks",74.821752943222862,{"$f":"F131*(1-Elteq!$F$4)","v":74.821752943222862}]
["ABTECH","BPG-EX 11","560 x 160 x  90","BPG-EX 11","1ks",113.82733267456892,{"$f":"F132*(1-Elteq!$F$4)","v":113.82733267456892}]
["ABTECH","BPG-EX 12","255 x 250 x 120","BPG-EX 12","1ks",93.958192060037931,{"$f":"F133*(1-Elteq!$F$4)","v":93.958192060037931}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ABTECH"},"BPG-EX 13","400 x 250 x 120","BPG-EX 13","1ks",136.45487892755969,{"$f":"F134*(1-Elteq!$F$4)","v":136.45487892755969}]
["ABTECH","BPG-EX 13.5","400 x 250 x 160","BPG-EX 13.5","1ks",255.05271999999999,{"$f":"F135*(1-Elteq!$F$4)","v":255.05271999999999}]
["ABTECH","BPG-EX 14","600 x 250 x 120","BPG-EX 14","1ks",229.29246869697332,{"$f":"F136*(1-Elteq!$F$4)","v":229.29246869697332}]
["ABTECH","BPG-EX 15","400 x 405 x 120","BPG-EX 15","1ks",158.34972368283459,{"$f":"F137*(1-Elteq!$F$4)","v":158.34972368283459}]

{"sheet":"ANAMET-M","index":2,"n_rows":2776,"n_cols":7,"rows_kept":2776,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["sheetname","Objednávací kód","Rozmer","Popis","Počet ks alebo m (malé balenie)","Cena za ks alebo m \n(malé balenie)","Cena po zľave za ks alebo m\n(malé balenie)"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},2560120,"M12 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",1,2.3876093367854945,{"$f":"F5*(1-Elteq!$F$5)","v":2.3876093367854945}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},2560150,"M16 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",1,2.3876093367854945,{"$f":"F6*(1-Elteq!$F$5)","v":2.3876093367854945}]
["ANAMET-M",2560160,"M16 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",1,2.7313507588129782,{"$f":"F7*(1-Elteq!$F$5)","v":2.7313507588129782}]
["ANAMET-M",2560170,"M20 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",1,2.9728987851025614,{"$f":"F8*(1-Elteq!$F$5)","v":2.9728987851025614}]
["ANAMET-M",2560200,"M20 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",1,3.5581882334196284,{"$f":"F9*(1-Elteq!$F$5)","v":3.5581882334196284}]
["ANAMET-M",2560250,"M25 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",1,5.1747019478191456,{"$f":"F10*(1-Elteq!$F$5)","v":5.1747019478191456}]
["ANAMET-M",2560320,"M32 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",1,9.0115994423421384,{"$f":"F11*(1-Elteq!$F$5)","v":9.0115994423421384}]
["ANAMET-M",2561120,"M12 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",1,3.0658018721370164,{"$f":"F12*(1-Elteq!$F$5)","v":3.0658018721370164}]
["ANAMET-M",2561150,"M16 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",1,3.2144468113921443,{"$f":"F13*(1-Elteq!$F$5)","v":3.2144468113921443}]
["ANAMET-M",2561160,"M16 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",1,3.2237371200955898,{"$f":"F14*(1-Elteq!$F$5)","v":3.2237371200955898}]
["ANAMET-M",2561170,"M20 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",1,3.6696719378609739,{"$f":"F15*(1-Elteq!$F$5)","v":3.6696719378609739}]
["ANAMET-M",2561200,"M20 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",1,4.4128966341366143,{"$f":"F16*(1-Elteq!$F$5)","v":4.4128966341366143}]
["ANAMET-M",2561250,"M25 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",1,6.6239901055566444,{"$f":"F17*(1-Elteq!$F$5)","v":6.6239901055566444}]
["ANAMET-M",2561320,"M32 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",1,11.715079275044781,{"$f":"F18*(1-Elteq!$F$5)","v":11.715079275044781}]
["ANAMET-M",2641120,"-","Multiflex fittings for FCEN, End cap, IP 40",1,1.5236106273650625,{"$f":"F19*(1-Elteq!$F$5)","v":1.5236106273650625}]
["ANAMET-M",2641160,"-","Multiflex fittings for FCEN, End cap, IP 40",1,1.9045132842063281,{"$f":"F20*(1-Elteq!$F$5)","v":1.9045132842063281}]
["ANAMET-M",2641200,"-","Multiflex fittings for FCEN, End cap, IP 40",1,2.3597384106751584,{"$f":"F21*(1-Elteq!$F$5)","v":2.3597384106751584}]
["ANAMET-M",2641250,"-","Multiflex fittings for FCEN, End cap, IP 40",1,3.2887692810197087,{"$f":"F22*(1-Elteq!$F$5)","v":3.2887692810197087}]
["ANAMET-M",2641320,"-","Multiflex fittings for FCEN, End cap, IP 40",1,4.8959926867157808,{"$f":"F23*(1-Elteq!$F$5)","v":4.8959926867157808}]
["ANAMET-M",7120143,"M20 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",1,5.6670883091017572,{"$f":"F24*(1-Elteq!$F$5)","v":5.6670883091017572}]
["ANAMET-M",7120153,"M16 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",1,5.3605081218880555,{"$f":"F25*(1-Elteq!$F$5)","v":5.3605081218880555}]
["ANAMET-M",7120163,"M16 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",1,4.3571547819159422,{"$f":"F26*(1-Elteq!$F$5)","v":4.3571547819159422}]
["ANAMET-M",7120173,"M20 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",1,4.663734969129643,{"$f":"F27*(1-Elteq!$F$5)","v":4.663734969129643}]
["ANAMET-M",7120203,"M20 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",1,4.9796054650467907,{"$f":"F28*(1-Elteq!$F$5)","v":4.9796054650467907}]
["ANAMET-M",7120253,"M25 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",1,7.3950857279426208,{"$f":"F29*(1-Elteq!$F$5)","v":7.3950857279426208}]
["ANAMET-M",7120323,"M32 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",1,12.337529958175629,{"$f":"F30*(1-Elteq!$F$5)","v":12.337529958175629}]
["ANAMET-M",8127153,"M16 x 1,5","Multiflex fittings for FCEN, Straight cablehose male thread, IP 68",1,12.922819406492696,{"$f":"F31*(1-Elteq!$F$5)","v":12.922819406492696}]
["ANAMET-M",8127163,"M16 x 1,5","Multiflex fittings for FCEN, Straight cablehose male thread, IP 68",1,15.384751212905755,{"$f":"F32*(1-Elteq!$F$5)","v":15.384751212905755}]
["ANAMET-M",8127173,"M20 x 1,5","Multiflex fittings for FCEN, Straight cablehose male thread, IP 68",1,13.03430311093404,{"$f":"F33*(1-Elteq!$F$5)","v":13.03430311093404}]
["ANAMET-M",8127203,"M20 x 1,5","Multiflex fittings for FCEN, Straight cablehose male thread, IP 68",1,17.595844684325787,{"$f":"F34*(1-Elteq!$F$5)","v":17.595844684325787}]
["ANAMET-M",8127253,"M25 x 1,5","Multiflex fittings for FCEN, Straight cablehose male thread, IP 68",1,24.563576211909915,{"$f":"F35*(1-Elteq!$F$5)","v":24.563576211909915}]
["ANAMET-M",8127323,"M32 x 1,5","Multiflex fittings for FCEN, Straight cablehose male thread, IP 68",1,61.873455964947055,{"$f":"F36*(1-Elteq!$F$5)","v":61.873455964947055}]
["ANAMET-M",8130153,"M16 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",1,9.5132761123281959,{"$f":"F37*(1-Elteq!$F$5)","v":9.5132761123281959}]
["ANAMET-M",8130163,"M16 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",1,8.8722448117904573,{"$f":"F38*(1-Elteq!$F$5)","v":8.8722448117904573}]
["ANAMET-M",8130203,"M20 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",1,10.052114017128035,{"$f":"F39*(1-Elteq!$F$5)","v":10.052114017128035}]
["ANAMET-M",8130253,"M25 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",1,13.16436743278228,{"$f":"F40*(1-Elteq!$F$5)","v":13.16436743278228}]
["ANAMET-M",8130323,"M32 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",1,22.371063357896773,{"$f":"F41*(1-Elteq!$F$5)","v":22.371063357896773}]
["ANAMET-M",8171120,"-","Multiflex fittings for FCEN, Connection set for FCEN",1,0.89186963553076837,{"$f":"F42*(1-Elteq!$F$5)","v":0.89186963553076837}]
["ANAMET-M",8171160,"-","Multiflex fittings for FCEN, Connection set for FCEN",1,1.0033533399721144,{"$f":"F43*(1-Elteq!$F$5)","v":1.0033533399721144}]
["ANAMET-M",8171200,"-","Multiflex fittings for FCEN, Connection set for FCEN",1,1.1148370444134605,{"$f":"F44*(1-Elteq!$F$5)","v":1.1148370444134605}]
["ANAMET-M",8171250,"-","Multiflex fittings for FCEN, Connection set for FCEN",1,1.3935463055168256,{"$f":"F45*(1-Elteq!$F$5)","v":1.3935463055168256}]
["ANAMET-M",8171320,"-","Multiflex fittings for FCEN, Connection set for FCEN",1,2.7870926110336511,{"$f":"F46*(1-Elteq!$F$5)","v":2.7870926110336511}]
["ANAMET-M",7100116,"PG 11","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,4.4128966341366143,{"$f":"F47*(1-Elteq!$F$5)","v":4.4128966341366143}]
["ANAMET-M",7100136,"PG 13,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,4.4221869428400593,{"$f":"F48*(1-Elteq!$F$5)","v":4.4221869428400593}]
["ANAMET-M",7100166,"PG 16","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,5.1468310217088087,{"$f":"F49*(1-Elteq!$F$5)","v":5.1468310217088087}]
["ANAMET-M",7100216,"PG 21","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,7.5158597410874126,{"$f":"F50*(1-Elteq!$F$5)","v":7.5158597410874126}]
["ANAMET-M",7100296,"PG 29","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,12.746303541127233,{"$f":"F51*(1-Elteq!$F$5)","v":12.746303541127233}]
["ANAMET-M",7100366,"PG 36","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,19.788357538338925,{"$f":"F52*(1-Elteq!$F$5)","v":19.788357538338925}]
["ANAMET-M",7120146,"M20 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,4.7752186735709889,{"$f":"F53*(1-Elteq!$F$5)","v":4.7752186735709889}]
["ANAMET-M",7120156,"M16 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,4.4686384863572872,{"$f":"F54*(1-Elteq!$F$5)","v":4.4686384863572872}]
["ANAMET-M",7120166,"M16 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,4.3571547819159422,{"$f":"F55*(1-Elteq!$F$5)","v":4.3571547819159422}]
["ANAMET-M",7120176,"M20 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,4.663734969129643,{"$f":"F56*(1-Elteq!$F$5)","v":4.663734969129643}]
["ANAMET-M",7120206,"M20 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,4.9796054650467907,{"$f":"F57*(1-Elteq!$F$5)","v":4.9796054650467907}]
["ANAMET-M",7120256,"M25 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,7.3950857279426208,{"$f":"F58*(1-Elteq!$F$5)","v":7.3950857279426208}]
["ANAMET-M",7120326,"M32 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,12.337529958175629,{"$f":"F59*(1-Elteq!$F$5)","v":12.337529958175629}]
["ANAMET-M",7120406,"M40 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,19.639712599083797,{"$f":"F60*(1-Elteq!$F$5)","v":19.639712599083797}]
["ANAMET-M",7129146,"M20 x 1,5","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",1,9.0952122206731474,{"$f":"F61*(1-Elteq!$F$5)","v":9.0952122206731474}]
["ANAMET-M",7129156,"M16 x 1,5","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",1,7.2371504799840478,{"$f":"F62*(1-Elteq!$F$5)","v":7.2371504799840478}]
["ANAMET-M",7129166,"M16 x 1,5","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",1,7.032763688508247,{"$f":"F63*(1-Elteq!$F$5)","v":7.032763688508247}]
["ANAMET-M",7129176,"M20 x 1,5","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",1,8.0918588807010359,{"$f":"F64*(1-Elteq!$F$5)","v":8.0918588807010359}]
["ANAMET-M",7129206,"M20 x 1,5","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",1,8.3055359808802809,{"$f":"F65*(1-Elteq!$F$5)","v":8.3055359808802809}]
["ANAMET-M",7129256,"M25 x 1,5","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",1,12.764884158534123,{"$f":"F66*(1-Elteq!$F$5)","v":12.764884158534123}]
["ANAMET-M",7129326,"M32 x 1,5","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",1,23.485900402310236,{"$f":"F67*(1-Elteq!$F$5)","v":23.485900402310236}]
["ANAMET-M",7129406,"M40 x 1,5","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",1,37.458524692292272,{"$f":"F68*(1-Elteq!$F$5)","v":37.458524692292272}]
["ANAMET-M",8130156,"M16 x 1,5","Multiflex fittings for SL / SLI, Straight swivel with male thread, IP 40",1,9.5039858036247509,{"$f":"F69*(1-Elteq!$F$5)","v":9.5039858036247509}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8130166,"M16 x 1,5","Multiflex fittings for SL / SLI, Straight swivel with male thread, IP 40",1,8.8722448117904573,{"$f":"F70*(1-Elteq!$F$5)","v":8.8722448117904573}]
["ANAMET-M",8130206,"M20 x 1,5","Multiflex fittings for SL / SLI, Straight swivel with male thread, IP 40",1,10.052114017128035,{"$f":"F71*(1-Elteq!$F$5)","v":10.052114017128035}]
["ANAMET-M",8130256,"M25 x 1,5","Multiflex fittings for SL / SLI, Straight swivel with male thread, IP 40",1,17.623715610436118,{"$f":"F72*(1-Elteq!$F$5)","v":17.623715610436118}]
["ANAMET-M",8130326,"M32 x 1,5","Multiflex fittings for SL / SLI, Straight swivel with male thread, IP 40",1,22.371063357896773,{"$f":"F73*(1-Elteq!$F$5)","v":22.371063357896773}]
["ANAMET-M",8130406,"M40 x 1,5","Multiflex fittings for SL / SLI, Straight swivel with male thread, IP 40",1,26.848992152957504,{"$f":"F74*(1-Elteq!$F$5)","v":26.848992152957504}]
["ANAMET-M",8139156,"M16 x 1,5","Multiflex fittings for SL / SLI, 90° elbow swivel with male thread, IP 40",1,16.564620418243333,{"$f":"F75*(1-Elteq!$F$5)","v":16.564620418243333}]
["ANAMET-M",8139166,"M16 x 1,5","Multiflex fittings for SL / SLI, 90° elbow swivel with male thread, IP 40",1,14.827332690699025,{"$f":"F76*(1-Elteq!$F$5)","v":14.827332690699025}]
["ANAMET-M",8139206,"M20 x 1,5","Multiflex fittings for SL / SLI, 90° elbow swivel with male thread, IP 40",1,19.017261915952947,{"$f":"F77*(1-Elteq!$F$5)","v":19.017261915952947}]
["ANAMET-M",8139256,"M20 x 1,5","Multiflex fittings for SL / SLI, 90° elbow swivel with male thread, IP 40",1,30.147051742680663,{"$f":"F78*(1-Elteq!$F$5)","v":30.147051742680663}]
["ANAMET-M",8139326,"M25 x 1,5","Multiflex fittings for SL / SLI, 90° elbow swivel with male thread, IP 40",1,49.071410571599152,{"$f":"F79*(1-Elteq!$F$5)","v":49.071410571599152}]
["ANAMET-M",8172106,"M32 x 1,5","Multiflex fittings for SL / SLI, Connection ring SL / SLI",1,0.89186963553076837,{"$f":"F80*(1-Elteq!$F$5)","v":0.89186963553076837}]
["ANAMET-M",8172136,"-","Multiflex fittings for SL / SLI, Connection ring SL / SLI",1,1.0033533399721144,{"$f":"F81*(1-Elteq!$F$5)","v":1.0033533399721144}]
["ANAMET-M",8172166,"-","Multiflex fittings for SL / SLI, Connection ring SL / SLI",1,1.1148370444134605,{"$f":"F82*(1-Elteq!$F$5)","v":1.1148370444134605}]
["ANAMET-M",8172206,"-","Multiflex fittings for SL / SLI, Connection ring SL / SLI",1,1.3935463055168256,{"$f":"F83*(1-Elteq!$F$5)","v":1.3935463055168256}]
["ANAMET-M",8172266,"-","Multiflex fittings for SL / SLI, Connection ring SL / SLI",1,2.7870926110336511,{"$f":"F84*(1-Elteq!$F$5)","v":2.7870926110336511}]
["ANAMET-M",8172356,"-","Multiflex fittings for SL / SLI, Connection ring SL / SLI",1,4.2363807687711494,{"$f":"F85*(1-Elteq!$F$5)","v":4.2363807687711494}]
["ANAMET-M",7109116,"PG 11","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",1,7.2836020235012748,{"$f":"F86*(1-Elteq!$F$5)","v":7.2836020235012748}]
["ANAMET-M",7109136,"PG 13,5","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",1,7.4786985062736315,{"$f":"F87*(1-Elteq!$F$5)","v":7.4786985062736315}]
["ANAMET-M",7109166,"PG 16","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",1,8.7886320334594465,{"$f":"F88*(1-Elteq!$F$5)","v":8.7886320334594465}]
["ANAMET-M",7109216,"PG 21","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",1,12.634819836685885,{"$f":"F89*(1-Elteq!$F$5)","v":12.634819836685885}]
["ANAMET-M",7109296,"PG 29","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",1,23.783190280820492,{"$f":"F90*(1-Elteq!$F$5)","v":23.783190280820492}]
["ANAMET-M",7109366,"PG 36","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",1,37.458524692292272,{"$f":"F91*(1-Elteq!$F$5)","v":37.458524692292272}]
["ANAMET-M",7140126,"NPT 1/2\"","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,4.5336706472814061,{"$f":"F92*(1-Elteq!$F$5)","v":4.5336706472814061}]
["ANAMET-M",7140166,"NPT 1/2\"","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,5.1654116391156997,{"$f":"F93*(1-Elteq!$F$5)","v":5.1654116391156997}]
["ANAMET-M",7140206,"NPT 3/4\"","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,7.0699249233220289,{"$f":"F94*(1-Elteq!$F$5)","v":7.0699249233220289}]
["ANAMET-M",7140266,"NPT 1\"","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,12.764884158534123,{"$f":"F95*(1-Elteq!$F$5)","v":12.764884158534123}]
["ANAMET-M",7140356,"NPT 1.1/4\"","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,20.466550073690449,{"$f":"F96*(1-Elteq!$F$5)","v":20.466550073690449}]
["ANAMET-M",7149126,"NPT 1/2\"","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",1,7.5716015933080856,{"$f":"F97*(1-Elteq!$F$5)","v":7.5716015933080856}]
["ANAMET-M",7149166,"NPT 1/2\"","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",1,8.9279866640111276,{"$f":"F98*(1-Elteq!$F$5)","v":8.9279866640111276}]
["ANAMET-M",7149206,"NPT 3/4\"","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",1,12.560497367058321,{"$f":"F99*(1-Elteq!$F$5)","v":12.560497367058321}]
["ANAMET-M",7149266,"NPT 1\"","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",1,23.485900402310236,{"$f":"F100*(1-Elteq!$F$5)","v":23.485900402310236}]
["ANAMET-M",7149356,"NPT 1.1/4\"","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",1,37.458524692292272,{"$f":"F101*(1-Elteq!$F$5)","v":37.458524692292272}]
["ANAMET-M",7840106,"-","Multiflex fittings for SL / SLI, Conduit connector, IP 40",1,8.3055359808802809,{"$f":"F102*(1-Elteq!$F$5)","v":8.3055359808802809}]
["ANAMET-M",7840126,"-","Multiflex fittings for SL / SLI, Conduit connector, IP 40",1,7.1906989364668199,{"$f":"F103*(1-Elteq!$F$5)","v":7.1906989364668199}]
["ANAMET-M",7840166,"-","Multiflex fittings for SL / SLI, Conduit connector, IP 40",1,8.6399870942043204,{"$f":"F104*(1-Elteq!$F$5)","v":8.6399870942043204}]
["ANAMET-M",7840206,"-","Multiflex fittings for SL / SLI, Conduit connector, IP 40",1,12.709142306313449,{"$f":"F105*(1-Elteq!$F$5)","v":12.709142306313449}]
["ANAMET-M",7840266,"-","Multiflex fittings for SL / SLI, Conduit connector, IP 40",1,23.086417128062081,{"$f":"F106*(1-Elteq!$F$5)","v":23.086417128062081}]
["ANAMET-M",7840356,"-","Multiflex fittings for SL / SLI, Conduit connector, IP 40",1,31.475565887273369,{"$f":"F107*(1-Elteq!$F$5)","v":31.475565887273369}]
["ANAMET-M",8100096,"PG 9","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,6.1316037442740328,{"$f":"F108*(1-Elteq!$F$5)","v":6.1316037442740328}]
["ANAMET-M",8100106,"PG 9","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,8.3426972156940646,{"$f":"F109*(1-Elteq!$F$5)","v":8.3426972156940646}]
["ANAMET-M",8100116,"PG 11","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,8.4913421549491908,{"$f":"F110*(1-Elteq!$F$5)","v":8.4913421549491908}]
["ANAMET-M",8100126,"PG 11","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,7.162828010356483,{"$f":"F111*(1-Elteq!$F$5)","v":7.162828010356483}]
["ANAMET-M",8100136,"PG 13,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,8.4913421549491908,{"$f":"F112*(1-Elteq!$F$5)","v":8.4913421549491908}]
["ANAMET-M",8100166,"PG 16","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,9.2903087034455041,{"$f":"F113*(1-Elteq!$F$5)","v":9.2903087034455041}]
["ANAMET-M",8100216,"PG 21","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,12.17030440151361,{"$f":"F114*(1-Elteq!$F$5)","v":12.17030440151361}]
["ANAMET-M",8100296,"PG 29","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,20.438679147580107,{"$f":"F115*(1-Elteq!$F$5)","v":20.438679147580107}]
["ANAMET-M",8100366,"PG 36","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,25.64125202150959,{"$f":"F116*(1-Elteq!$F$5)","v":25.64125202150959}]
["ANAMET-M",8103116,"PG 11","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",1,9.2159862338179401,{"$f":"F117*(1-Elteq!$F$5)","v":9.2159862338179401}]
["ANAMET-M",8103126,"PG 11","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",1,8.0825685719975873,{"$f":"F118*(1-Elteq!$F$5)","v":8.0825685719975873}]
["ANAMET-M",8103136,"PG 13,5","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",1,9.2159862338179401,{"$f":"F119*(1-Elteq!$F$5)","v":9.2159862338179401}]
["ANAMET-M",8103146,"PG 13,5","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",1,8.0825685719975873,{"$f":"F120*(1-Elteq!$F$5)","v":8.0825685719975873}]
["ANAMET-M",8103166,"PG 16","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",1,9.6619210515833238,{"$f":"F121*(1-Elteq!$F$5)","v":9.6619210515833238}]
["ANAMET-M",8103216,"PG 21","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",1,13.65675379406489,{"$f":"F122*(1-Elteq!$F$5)","v":13.65675379406489}]
["ANAMET-M",8103296,"PG 29","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",1,19.974163712407837,{"$f":"F123*(1-Elteq!$F$5)","v":19.974163712407837}]
["ANAMET-M",8103366,"PG 36","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",1,32.841241266679859,{"$f":"F124*(1-Elteq!$F$5)","v":32.841241266679859}]
["ANAMET-M",8107096,"PG 9","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",1,14.474300959968096,{"$f":"F125*(1-Elteq!$F$5)","v":14.474300959968096}]
["ANAMET-M",8107116,"PG 11","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",1,15.477654299940209,{"$f":"F126*(1-Elteq!$F$5)","v":15.477654299940209}]
["ANAMET-M",8107126,"PG 9","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",1,15.477654299940209,{"$f":"F127*(1-Elteq!$F$5)","v":15.477654299940209}]
["ANAMET-M",8107146,"PG 11","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",1,14.344236638119858,{"$f":"F128*(1-Elteq!$F$5)","v":14.344236638119858}]
["ANAMET-M",8107156,"PG 13,5","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",1,17.354296658036201,{"$f":"F129*(1-Elteq!$F$5)","v":17.354296658036201}]
["ANAMET-M",8107166,"PG 16","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",1,21.014678287193732,{"$f":"F130*(1-Elteq!$F$5)","v":21.014678287193732}]
["ANAMET-M",8107216,"PG 21","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",1,32.200209966142111,{"$f":"F131*(1-Elteq!$F$5)","v":32.200209966142111}]
["ANAMET-M",8107296,"PG 29","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",1,48.43966957976486,{"$f":"F132*(1-Elteq!$F$5)","v":48.43966957976486}]
["ANAMET-M",8120146,"M20 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,7.7295368412666594,{"$f":"F133*(1-Elteq!$F$5)","v":7.7295368412666594}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8120156,"M16 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,5.8714751005775589,{"$f":"F134*(1-Elteq!$F$5)","v":5.8714751005775589}]
["ANAMET-M",8120166,"M16 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,8.036117028480362,{"$f":"F135*(1-Elteq!$F$5)","v":8.036117028480362}]
["ANAMET-M",8120176,"M20 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,8.3798584505078431,{"$f":"F136*(1-Elteq!$F$5)","v":8.3798584505078431}]
["ANAMET-M",8120206,"M20 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,8.3798584505078431,{"$f":"F137*(1-Elteq!$F$5)","v":8.3798584505078431}]
["ANAMET-M",8120256,"M25 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,11.724369583748224,{"$f":"F138*(1-Elteq!$F$5)","v":11.724369583748224}]
["ANAMET-M",8120326,"M32 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,19.045132842063285,{"$f":"F139*(1-Elteq!$F$5)","v":19.045132842063285}]
["ANAMET-M",8120406,"M40 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",1,25.64125202150959,{"$f":"F140*(1-Elteq!$F$5)","v":25.64125202150959}]
["ANAMET-M",8123156,"M16 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",1,7.8131496195976684,{"$f":"F141*(1-Elteq!$F$5)","v":7.8131496195976684}]
["ANAMET-M",8123166,"M16 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",1,8.9558575901214663,{"$f":"F142*(1-Elteq!$F$5)","v":8.9558575901214663}]
["ANAMET-M",8123206,"M20 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",1,9.364631173073068,{"$f":"F143*(1-Elteq!$F$5)","v":9.364631173073068}]
["ANAMET-M",8123256,"M25 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",1,13.173657741485725,{"$f":"F144*(1-Elteq!$F$5)","v":13.173657741485725}]
["ANAMET-M",8123326,"M32 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",1,19.268100250945974,{"$f":"F145*(1-Elteq!$F$5)","v":19.268100250945974}]
["ANAMET-M",8123406,"M40 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",1,32.841241266679859,{"$f":"F146*(1-Elteq!$F$5)","v":32.841241266679859}]
["ANAMET-M",8127156,"M16 x 1,5","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",1,12.913529097789251,{"$f":"F147*(1-Elteq!$F$5)","v":12.913529097789251}]
["ANAMET-M",8127166,"M16 x 1,5","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",1,15.477654299940209,{"$f":"F148*(1-Elteq!$F$5)","v":15.477654299940209}]
["ANAMET-M",8127176,"M20 x 1,5","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",1,15.477654299940209,{"$f":"F149*(1-Elteq!$F$5)","v":15.477654299940209}]
["ANAMET-M",8127206,"M20 x 1,5","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",1,17.354296658036201,{"$f":"F150*(1-Elteq!$F$5)","v":17.354296658036201}]
["ANAMET-M",8127256,"M25 x 1,5","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",1,27.629378084046927,{"$f":"F151*(1-Elteq!$F$5)","v":27.629378084046927}]
["ANAMET-M",8127326,"M32 x 1,5","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",1,65.886869324835516,{"$f":"F152*(1-Elteq!$F$5)","v":65.886869324835516}]
["ANAMET-M",8127406,"M40 x 1,5","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",1,82.154199864568611,{"$f":"F153*(1-Elteq!$F$5)","v":82.154199864568611}]
["ANAMET-M",8172106,"M32 x 1,5","Multiflex fittings for SL / SLI, Connection ring SL / SLI",1,0.89186963553076837,{"$f":"F154*(1-Elteq!$F$5)","v":0.89186963553076837}]
["ANAMET-M",8172356,"-","Multiflex fittings for SL / SLI, Connection ring SL / SLI",1,4.2363807687711494,{"$f":"F155*(1-Elteq!$F$5)","v":4.2363807687711494}]
["ANAMET-M",8173126,"-","Multiflex fittings for SL / SLI, Connection set for SL / SLI",1,3.455994837681728,{"$f":"F156*(1-Elteq!$F$5)","v":3.455994837681728}]
["ANAMET-M",8173166,"-","Multiflex fittings for SL / SLI, Connection set for SL / SLI",1,3.455994837681728,{"$f":"F157*(1-Elteq!$F$5)","v":3.455994837681728}]
["ANAMET-M",8173206,"-","Multiflex fittings for SL / SLI, Connection set for SL / SLI",1,4.4593481776538422,{"$f":"F158*(1-Elteq!$F$5)","v":4.4593481776538422}]
["ANAMET-M",8173266,"-","Multiflex fittings for SL / SLI, Connection set for SL / SLI",1,6.8005059709221092,{"$f":"F159*(1-Elteq!$F$5)","v":6.8005059709221092}]
["ANAMET-M",8172106,"M32 x 1,5","Multiflex fittings for SL / SLI, Connection ring SL / SLI",1,0.89186963553076837,{"$f":"F160*(1-Elteq!$F$5)","v":0.89186963553076837}]
["ANAMET-M",8172136,"-","Multiflex fittings for SL / SLI, Connection ring SL / SLI",1,1.0033533399721144,{"$f":"F161*(1-Elteq!$F$5)","v":1.0033533399721144}]
["ANAMET-M",8172166,"-","Multiflex fittings for SL / SLI, Connection ring SL / SLI",1,1.1148370444134605,{"$f":"F162*(1-Elteq!$F$5)","v":1.1148370444134605}]
["ANAMET-M",8172206,"-","Multiflex fittings for SL / SLI, Connection ring SL / SLI",1,1.3935463055168256,{"$f":"F163*(1-Elteq!$F$5)","v":1.3935463055168256}]
["ANAMET-M",8172266,"-","Multiflex fittings for SL / SLI, Connection ring SL / SLI",1,2.7870926110336511,{"$f":"F164*(1-Elteq!$F$5)","v":2.7870926110336511}]
["ANAMET-M",8172356,"-","Multiflex fittings for SL / SLI, Connection ring SL / SLI",1,4.2363807687711494,{"$f":"F165*(1-Elteq!$F$5)","v":4.2363807687711494}]
["ANAMET-M","7120169-6","M16 x 1,5","Stainless steel 304 fittings SLI, Straight fixed with male thread, IP 40",1,18.970810372435722,{"$f":"F166*(1-Elteq!$F$5)","v":18.970810372435722}]
["ANAMET-M","7120179-6","M20 x 1,5","Stainless steel 304 fittings SLI, Straight fixed with male thread, IP 40",1,25.316091216888999,{"$f":"F167*(1-Elteq!$F$5)","v":25.316091216888999}]
["ANAMET-M","7120209-6","M20 x 1,5","Stainless steel 304 fittings SLI, Straight fixed with male thread, IP 40",1,25.427574921330347,{"$f":"F168*(1-Elteq!$F$5)","v":25.427574921330347}]
["ANAMET-M","7120259-6","M25 x 1,5","Stainless steel 304 fittings SLI, Straight fixed with male thread, IP 40",1,30.332857916749571,{"$f":"F169*(1-Elteq!$F$5)","v":30.332857916749571}]
["ANAMET-M","7120329-6","M32 x 1,5","Stainless steel 304 fittings SLI, Straight fixed with male thread, IP 40",1,38.852070997809101,{"$f":"F170*(1-Elteq!$F$5)","v":38.852070997809101}]
["ANAMET-M","7120409-6","M40 x 1,5","Stainless steel 304 fittings SLI, Straight fixed with male thread, IP 40",1,57.507010874327669,{"$f":"F171*(1-Elteq!$F$5)","v":57.507010874327669}]
["ANAMET-M","7129169-6","M16 x 1,5","Stainless steel 304 fittings SLI, 90° elbow fixed with male thread, IP 40",1,37.235557283409577,{"$f":"F172*(1-Elteq!$F$5)","v":37.235557283409577}]
["ANAMET-M","7129179-6","M20 x 1,5","Stainless steel 304 fittings SLI, 90° elbow fixed with male thread, IP 40",1,38.350394327823039,{"$f":"F173*(1-Elteq!$F$5)","v":38.350394327823039}]
["ANAMET-M","7129209-6","M20 x 1,5","Stainless steel 304 fittings SLI, 90° elbow fixed with male thread, IP 40",1,42.252323983270152,{"$f":"F174*(1-Elteq!$F$5)","v":42.252323983270152}]
["ANAMET-M","7129259-6","M25 x 1,5","Stainless steel 304 fittings SLI, 90° elbow fixed with male thread, IP 40",1,54.348305915156196,{"$f":"F175*(1-Elteq!$F$5)","v":54.348305915156196}]
["ANAMET-M","7129329-6","M32 x 1,5","Stainless steel 304 fittings SLI, 90° elbow fixed with male thread, IP 40",1,82.274973877713393,{"$f":"F176*(1-Elteq!$F$5)","v":82.274973877713393}]
["ANAMET-M","7129409-6","M40 x 1,5","Stainless steel 304 fittings SLI, 90° elbow fixed with male thread, IP 40",1,106.24397033260279,{"$f":"F177*(1-Elteq!$F$5)","v":106.24397033260279}]
["ANAMET-M","7140129-6","NPT 1/2\"","Stainless steel 304 fittings SLI, Straight fixed with male thread, IP 40",1,18.970810372435722,{"$f":"F178*(1-Elteq!$F$5)","v":18.970810372435722}]
["ANAMET-M","7140169-6","NPT 1/2\"","Stainless steel 304 fittings SLI, Straight fixed with male thread, IP 40",1,25.427574921330347,{"$f":"F179*(1-Elteq!$F$5)","v":25.427574921330347}]
["ANAMET-M","7140209-6","NPT 3/4\"","Stainless steel 304 fittings SLI, Straight fixed with male thread, IP 40",1,30.332857916749571,{"$f":"F180*(1-Elteq!$F$5)","v":30.332857916749571}]
["ANAMET-M","7140269-6","NPT 1\"","Stainless steel 304 fittings SLI, Straight fixed with male thread, IP 40",1,38.852070997809101,{"$f":"F181*(1-Elteq!$F$5)","v":38.852070997809101}]
["ANAMET-M","7140359-6","NPT 1.1/4\"","Stainless steel 304 fittings SLI, Straight fixed with male thread, IP 40",1,57.507010874327669,{"$f":"F182*(1-Elteq!$F$5)","v":57.507010874327669}]
["ANAMET-M","7149129-6","NPT 1/2\"","Stainless steel 304 fittings SLI, 90° elbow fixed with male thread, IP 40",1,37.235557283409577,{"$f":"F183*(1-Elteq!$F$5)","v":37.235557283409577}]
["ANAMET-M","7149169-6","NPT 1/2\"","Stainless steel 304 fittings SLI, 90° elbow fixed with male thread, IP 40",1,42.252323983270152,{"$f":"F184*(1-Elteq!$F$5)","v":42.252323983270152}]
["ANAMET-M","7149209-6","NPT 3/4\"","Stainless steel 304 fittings SLI, 90° elbow fixed with male thread, IP 40",1,54.348305915156196,{"$f":"F185*(1-Elteq!$F$5)","v":54.348305915156196}]
["ANAMET-M","7149269-6","NPT 1\"","Stainless steel 304 fittings SLI, 90° elbow fixed with male thread, IP 40",1,82.274973877713393,{"$f":"F186*(1-Elteq!$F$5)","v":82.274973877713393}]
["ANAMET-M","7149359-6","NPT 1.1/4\"","Stainless steel 304 fittings SLI, 90° elbow fixed with male thread, IP 40",1,106.24397033260279,{"$f":"F187*(1-Elteq!$F$5)","v":106.24397033260279}]
["ANAMET-M",2605070,"PG 7","Multiflex fittings for SLI - CAP, Straight fixed with male thread, IP 40",1,5.1747019478191456,{"$f":"F188*(1-Elteq!$F$5)","v":5.1747019478191456}]
["ANAMET-M",2605090,"PG 9","Multiflex fittings for SLI - CAP, Straight fixed with male thread, IP 40",1,5.5277336785500752,{"$f":"F189*(1-Elteq!$F$5)","v":5.5277336785500752}]
["ANAMET-M",2605120,"M12 x 1,5","Multiflex fittings for SLI - CAP, Straight fixed with male thread, IP 40",1,5.5277336785500752,{"$f":"F190*(1-Elteq!$F$5)","v":5.5277336785500752}]
["ANAMET-M",2605130,"M16 x 1,5","Multiflex fittings for SLI - CAP, Straight fixed with male thread, IP 40",1,4.8123799083847709,{"$f":"F191*(1-Elteq!$F$5)","v":4.8123799083847709}]
["ANAMET-M",2615070,"PG 7","Multiflex fittings for SLI - CAP, Straight swivel with male thread, IP 40",1,5.9457975702051229,{"$f":"F192*(1-Elteq!$F$5)","v":5.9457975702051229}]
["ANAMET-M",2615090,"PG 9","Multiflex fittings for SLI - CAP, Straight swivel with male thread, IP 40",1,7.3579244931288388,{"$f":"F193*(1-Elteq!$F$5)","v":7.3579244931288388}]
["ANAMET-M",2615120,"M12 x 1,5","Multiflex fittings for SLI - CAP, Straight swivel with male thread, IP 40",1,7.8596011631148972,{"$f":"F194*(1-Elteq!$F$5)","v":7.8596011631148972}]
["ANAMET-M",2615130,"M16 x 1,5","Multiflex fittings for SLI - CAP, Straight swivel with male thread, IP 40",1,6.8562478231427821,{"$f":"F195*(1-Elteq!$F$5)","v":6.8562478231427821}]
["ANAMET-M",8100072,"PG 7","Multiflex fittings for SLI - CAP, Straight fixed with male thread, IP 40",1,5.2397341087432645,{"$f":"F196*(1-Elteq!$F$5)","v":5.2397341087432645}]
["ANAMET-M",8100092,"PG 9","Multiflex fittings for SLI - CAP, Straight fixed with male thread, IP 40",1,5.2397341087432645,{"$f":"F197*(1-Elteq!$F$5)","v":5.2397341087432645}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8120112,"M12 x 1,5","Multiflex fittings for SLI - CAP, Straight fixed with male thread, IP 40",1,5.4069596654052834,{"$f":"F198*(1-Elteq!$F$5)","v":5.4069596654052834}]
["ANAMET-M",8120122,"M12 x 1,5","Multiflex fittings for SLI - CAP, Straight fixed with male thread, IP 40",1,5.2397341087432645,{"$f":"F199*(1-Elteq!$F$5)","v":5.2397341087432645}]
["ANAMET-M",8120132,"M16 x 1,5","Multiflex fittings for SLI - CAP, Straight fixed with male thread, IP 40",1,5.2397341087432645,{"$f":"F200*(1-Elteq!$F$5)","v":5.2397341087432645}]
["ANAMET-M",8120142,"M20 x 1,5","Multiflex fittings for SLI - CAP, Straight fixed with male thread, IP 40",1,5.4069596654052834,{"$f":"F201*(1-Elteq!$F$5)","v":5.4069596654052834}]
["ANAMET-M",8120152,"M16 x 1,5","Multiflex fittings for SLI - CAP, Straight fixed with male thread, IP 40",1,4.9796054650467907,{"$f":"F202*(1-Elteq!$F$5)","v":4.9796054650467907}]
["ANAMET-M",8172066,"-","Multiflex fittings for SLI - CAP, Connection set for SLI-CAP",1,0.89186963553076837,{"$f":"F203*(1-Elteq!$F$5)","v":0.89186963553076837}]
["ANAMET-M",8172096,"-","Multiflex fittings for SLI - CAP, Connection set for SLI-CAP",1,0.98477272256522352,{"$f":"F204*(1-Elteq!$F$5)","v":0.98477272256522352}]
["ANAMET-M",7120140,"M20 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",1,4.7752186735709889,{"$f":"F205*(1-Elteq!$F$5)","v":4.7752186735709889}]
["ANAMET-M",7120150,"M16 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",1,4.4686384863572872,{"$f":"F206*(1-Elteq!$F$5)","v":4.4686384863572872}]
["ANAMET-M",7120161,"M16 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",1,3.3538014419438267,{"$f":"F207*(1-Elteq!$F$5)","v":3.3538014419438267}]
["ANAMET-M",7120171,"M20 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",1,3.6603816291575288,{"$f":"F208*(1-Elteq!$F$5)","v":3.6603816291575288}]
["ANAMET-M",7120201,"M20 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",1,3.8647684206333297,{"$f":"F209*(1-Elteq!$F$5)","v":3.8647684206333297}]
["ANAMET-M",7120251,"M25 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",1,6.0015394224257959,{"$f":"F210*(1-Elteq!$F$5)","v":6.0015394224257959}]
["ANAMET-M",7120321,"M32 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",1,9.5504373471419779,{"$f":"F211*(1-Elteq!$F$5)","v":9.5504373471419779}]
["ANAMET-M",7120401,"M40 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",1,15.403331830312645,{"$f":"F212*(1-Elteq!$F$5)","v":15.403331830312645}]
["ANAMET-M",7120501,"M50 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",1,21.627838661621134,{"$f":"F213*(1-Elteq!$F$5)","v":21.627838661621134}]
["ANAMET-M",7120631,"M63 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",1,30.992469834694202,{"$f":"F214*(1-Elteq!$F$5)","v":30.992469834694202}]
["ANAMET-M",8120161,"M16 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",1,4.5801221907986331,{"$f":"F215*(1-Elteq!$F$5)","v":4.5801221907986331}]
["ANAMET-M",8120171,"M20 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",1,4.9238636128261177,{"$f":"F216*(1-Elteq!$F$5)","v":4.9238636128261177}]
["ANAMET-M",8120201,"M20 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",1,4.9238636128261177,{"$f":"F217*(1-Elteq!$F$5)","v":4.9238636128261177}]
["ANAMET-M",8120251,"M25 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",1,7.2650214060943847,{"$f":"F218*(1-Elteq!$F$5)","v":7.2650214060943847}]
["ANAMET-M",8120321,"M32 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",1,11.61288587930688,{"$f":"F219*(1-Elteq!$F$5)","v":11.61288587930688}]
["ANAMET-M",8120401,"M40 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",1,21.414161561441887,{"$f":"F220*(1-Elteq!$F$5)","v":21.414161561441887}]
["ANAMET-M",8120501,"M50 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",1,28.734924819756944,{"$f":"F221*(1-Elteq!$F$5)","v":28.734924819756944}]
["ANAMET-M",8120631,"M63 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",1,44.063934180442025,{"$f":"F222*(1-Elteq!$F$5)","v":44.063934180442025}]
["ANAMET-M",8177100,"-","Multiflex fittings for SLB, Connection set for SLB",1,1.5607718621788444,{"$f":"F223*(1-Elteq!$F$5)","v":1.5607718621788444}]
["ANAMET-M",8177120,"-","Multiflex fittings for SLB, Connection set for SLB",1,1.5607718621788444,{"$f":"F224*(1-Elteq!$F$5)","v":1.5607718621788444}]
["ANAMET-M",8177160,"-","Multiflex fittings for SLB, Connection set for SLB",1,1.7837392710615367,{"$f":"F225*(1-Elteq!$F$5)","v":1.7837392710615367}]
["ANAMET-M",8177200,"-","Multiflex fittings for SLB, Connection set for SLB",1,2.2296740888269211,{"$f":"F226*(1-Elteq!$F$5)","v":2.2296740888269211}]
["ANAMET-M",8177260,"-","Multiflex fittings for SLB, Connection set for SLB",1,2.8985763154749975,{"$f":"F227*(1-Elteq!$F$5)","v":2.8985763154749975}]
["ANAMET-M",8177350,"-","Multiflex fittings for SLB, Connection set for SLB",1,3.3445111332403816,{"$f":"F228*(1-Elteq!$F$5)","v":3.3445111332403816}]
["ANAMET-M",8177400,"-","Multiflex fittings for SLB, Connection set for SLB",1,4.682315586536534,{"$f":"F229*(1-Elteq!$F$5)","v":4.682315586536534}]
["ANAMET-M",8177500,"-","Multiflex fittings for SLB, Connection set for SLB",1,7.3579244931288388,{"$f":"F230*(1-Elteq!$F$5)","v":7.3579244931288388}]
["ANAMET-M",8172109,"-","Multiflex fittings for UI / UIG, Connection set for UI",1,2.5641252021509588,{"$f":"F231*(1-Elteq!$F$5)","v":2.5641252021509588}]
["ANAMET-M",8172139,"-","Multiflex fittings for UI / UIG, Connection set for UI",1,2.7870926110336511,{"$f":"F232*(1-Elteq!$F$5)","v":2.7870926110336511}]
["ANAMET-M",8172169,"-","Multiflex fittings for UI / UIG, Connection set for UI",1,3.6232203943437464,{"$f":"F233*(1-Elteq!$F$5)","v":3.6232203943437464}]
["ANAMET-M",8172209,"-","Multiflex fittings for UI / UIG, Connection set for UI",1,5.4627015176259563,{"$f":"F234*(1-Elteq!$F$5)","v":5.4627015176259563}]
["ANAMET-M",8172269,"-","Multiflex fittings for UI / UIG, Connection set for UI",1,9.4761148775144139,{"$f":"F235*(1-Elteq!$F$5)","v":9.4761148775144139}]
["ANAMET-M",8172359,"-","Multiflex fittings for UI / UIG, Connection set for UI",1,10.145017104162491,{"$f":"F236*(1-Elteq!$F$5)","v":10.145017104162491}]
["ANAMET-M",8172406,"-","Multiflex fittings for UI / UIG, Connection ring for UIG",1,6.6890222664807633,{"$f":"F237*(1-Elteq!$F$5)","v":6.6890222664807633}]
["ANAMET-M",8172409,"-","Multiflex fittings for UI / UIG, Connection set for UI",1,19.17519716391152,{"$f":"F238*(1-Elteq!$F$5)","v":19.17519716391152}]
["ANAMET-M",8172506,"-","Multiflex fittings for UI / UIG, Connection ring for UIG",1,8.0268267197769152,{"$f":"F239*(1-Elteq!$F$5)","v":8.0268267197769152}]
["ANAMET-M",8172509,"-","Multiflex fittings for UI / UIG, Connection set for UI",1,19.844099390559595,{"$f":"F240*(1-Elteq!$F$5)","v":19.844099390559595}]
["ANAMET-M",7100117,"PG 11","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,6.1966359051981517,{"$f":"F241*(1-Elteq!$F$5)","v":6.1966359051981517}]
["ANAMET-M",7100137,"PG 13,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,6.2059262139015967,{"$f":"F242*(1-Elteq!$F$5)","v":6.2059262139015967}]
["ANAMET-M",7100167,"PG 16","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,7.6552143716390955,{"$f":"F243*(1-Elteq!$F$5)","v":7.6552143716390955}]
["ANAMET-M",7100217,"PG 21","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,11.5757246444931,{"$f":"F244*(1-Elteq!$F$5)","v":11.5757246444931}]
["ANAMET-M",7100297,"PG 29","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,19.435325807607995,{"$f":"F245*(1-Elteq!$F$5)","v":19.435325807607995}]
["ANAMET-M",7100367,"PG 36","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,25.696993873730264,{"$f":"F246*(1-Elteq!$F$5)","v":25.696993873730264}]
["ANAMET-M",7100427,"PG 42","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,28.214667532363997,{"$f":"F247*(1-Elteq!$F$5)","v":28.214667532363997}]
["ANAMET-M",7100487,"PG 48","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,38.805619454291872,{"$f":"F248*(1-Elteq!$F$5)","v":38.805619454291872}]
["ANAMET-M",7109117,"PG 11","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,8.8443738856801186,{"$f":"F249*(1-Elteq!$F$5)","v":8.8443738856801186}]
["ANAMET-M",7109137,"PG 13,5","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,9.0394703684524753,{"$f":"F250*(1-Elteq!$F$5)","v":9.0394703684524753}]
["ANAMET-M",7109167,"PG 16","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,10.460887600079637,{"$f":"F251*(1-Elteq!$F$5)","v":10.460887600079637}]
["ANAMET-M",7109217,"PG 21","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,14.864493925512807,{"$f":"F252*(1-Elteq!$F$5)","v":14.864493925512807}]
["ANAMET-M",7109297,"PG 29","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,26.458799187412794,{"$f":"F253*(1-Elteq!$F$5)","v":26.458799187412794}]
["ANAMET-M",7109367,"PG 36","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,42.698258801035536,{"$f":"F254*(1-Elteq!$F$5)","v":42.698258801035536}]
["ANAMET-M",7109427,"PG 42","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,63.945194805815397,{"$f":"F255*(1-Elteq!$F$5)","v":63.945194805815397}]
["ANAMET-M",7109487,"PG 48","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,89.595737136028433,{"$f":"F256*(1-Elteq!$F$5)","v":89.595737136028433}]
["ANAMET-M",7120147,"M20 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,6.4474742401911795,{"$f":"F257*(1-Elteq!$F$5)","v":6.4474742401911795}]
["ANAMET-M",7120157,"M16 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,6.1408940529774787,{"$f":"F258*(1-Elteq!$F$5)","v":6.1408940529774787}]
["ANAMET-M",7120167,"M16 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,6.1408940529774787,{"$f":"F259*(1-Elteq!$F$5)","v":6.1408940529774787}]
["ANAMET-M",7120177,"M20 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,6.4474742401911795,{"$f":"F260*(1-Elteq!$F$5)","v":6.4474742401911795}]
["ANAMET-M",7120207,"M20 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,7.4879888149770775,{"$f":"F261*(1-Elteq!$F$5)","v":7.4879888149770775}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},7120257,"M25 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,11.454950631348307,{"$f":"F262*(1-Elteq!$F$5)","v":11.454950631348307}]
["ANAMET-M",7120327,"M32 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,19.026552224656392,{"$f":"F263*(1-Elteq!$F$5)","v":19.026552224656392}]
["ANAMET-M",7120407,"M40 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,25.548348934475136,{"$f":"F264*(1-Elteq!$F$5)","v":25.548348934475136}]
["ANAMET-M",7120507,"M50 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,28.316860928101896,{"$f":"F265*(1-Elteq!$F$5)","v":28.316860928101896}]
["ANAMET-M",7120637,"M63 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,39.019296554471119,{"$f":"F266*(1-Elteq!$F$5)","v":39.019296554471119}]
["ANAMET-M",7129147,"M20 x 1,5","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,10.769325849034029,{"$f":"F267*(1-Elteq!$F$5)","v":10.769325849034029}]
["ANAMET-M",7129157,"M16 x 1,5","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,9.7083725951005508,{"$f":"F268*(1-Elteq!$F$5)","v":9.7083725951005508}]
["ANAMET-M",7129167,"M16 x 1,5","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,8.8165029595697835,{"$f":"F269*(1-Elteq!$F$5)","v":8.8165029595697835}]
["ANAMET-M",7129177,"M20 x 1,5","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,9.8755981517625724,{"$f":"F270*(1-Elteq!$F$5)","v":9.8755981517625724}]
["ANAMET-M",7129207,"M20 x 1,5","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,10.813919330810567,{"$f":"F271*(1-Elteq!$F$5)","v":10.813919330810567}]
["ANAMET-M",7129257,"M25 x 1,5","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,16.834039370643254,{"$f":"F272*(1-Elteq!$F$5)","v":16.834039370643254}]
["ANAMET-M",7129327,"M32 x 1,5","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,30.174922668790995,{"$f":"F273*(1-Elteq!$F$5)","v":30.174922668790995}]
["ANAMET-M",7129407,"M40 x 1,5","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,43.367161027683608,{"$f":"F274*(1-Elteq!$F$5)","v":43.367161027683608}]
["ANAMET-M",7129507,"M50 x 1,5","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,63.945194805815397,{"$f":"F275*(1-Elteq!$F$5)","v":63.945194805815397}]
["ANAMET-M",7129637,"M63 x 1,5","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,87.05948285998781,{"$f":"F276*(1-Elteq!$F$5)","v":87.05948285998781}]
["ANAMET-M",8130167,"M16 x 1,5","Multiflex fittings for UI / UIG, Straight swivel with male thread, IP 40",1,10.655984082851994,{"$f":"F277*(1-Elteq!$F$5)","v":10.655984082851994}]
["ANAMET-M",8130207,"M20 x 1,5","Multiflex fittings for UI / UIG, Straight swivel with male thread, IP 40",1,12.560497367058321,{"$f":"F278*(1-Elteq!$F$5)","v":12.560497367058321}]
["ANAMET-M",8130257,"M25 x 1,5","Multiflex fittings for UI / UIG, Straight swivel with male thread, IP 40",1,17.233522644891412,{"$f":"F279*(1-Elteq!$F$5)","v":17.233522644891412}]
["ANAMET-M",8130327,"M32 x 1,5","Multiflex fittings for UI / UIG, Straight swivel with male thread, IP 40",1,29.060085624377539,{"$f":"F280*(1-Elteq!$F$5)","v":29.060085624377539}]
["ANAMET-M",8130407,"M40 x 1,5","Multiflex fittings for UI / UIG, Straight swivel with male thread, IP 40",1,32.766918797052298,{"$f":"F281*(1-Elteq!$F$5)","v":32.766918797052298}]
["ANAMET-M",8130507,"M50 x 1,5","Multiflex fittings for UI / UIG, Straight swivel with male thread, IP 40",1,46.544446604261971,{"$f":"F282*(1-Elteq!$F$5)","v":46.544446604261971}]
["ANAMET-M",8130637,"M63 x 1,5","Multiflex fittings for UI / UIG, Straight swivel with male thread, IP 40",1,67.429060569607472,{"$f":"F283*(1-Elteq!$F$5)","v":67.429060569607472}]
["ANAMET-M",8139157,"M16 x 1,5","Multiflex fittings for UI / UIG, 90° elbow swivel with male thread, IP 40",1,18.236875984863524,{"$f":"F284*(1-Elteq!$F$5)","v":18.236875984863524}]
["ANAMET-M",8139167,"M20 x 1,5","Multiflex fittings for UI / UIG, 90° elbow swivel with male thread, IP 40",1,16.611071961760562,{"$f":"F285*(1-Elteq!$F$5)","v":16.611071961760562}]
["ANAMET-M",8139207,"M20 x 1,5","Multiflex fittings for UI / UIG, 90° elbow swivel with male thread, IP 40",1,21.525645265883234,{"$f":"F286*(1-Elteq!$F$5)","v":21.525645265883234}]
["ANAMET-M",8139257,"M25 x 1,5","Multiflex fittings for UI / UIG, 90° elbow swivel with male thread, IP 40",1,34.21620695478979,{"$f":"F287*(1-Elteq!$F$5)","v":34.21620695478979}]
["ANAMET-M",8139327,"M32 x 1,5","Multiflex fittings for UI / UIG, 90° elbow swivel with male thread, IP 40",1,55.760432838079915,{"$f":"F288*(1-Elteq!$F$5)","v":55.760432838079915}]
["ANAMET-M",7140127,"NPT 1/2\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,6.3174099183429426,{"$f":"F289*(1-Elteq!$F$5)","v":6.3174099183429426}]
["ANAMET-M",7140167,"NPT 1/2\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,7.6737949890459864,{"$f":"F290*(1-Elteq!$F$5)","v":7.6737949890459864}]
["ANAMET-M",7140207,"NPT 3/4\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,11.129789826727714,{"$f":"F291*(1-Elteq!$F$5)","v":11.129789826727714}]
["ANAMET-M",7140267,"NPT 1\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,19.453906425014885,{"$f":"F292*(1-Elteq!$F$5)","v":19.453906425014885}]
["ANAMET-M",7140357,"NPT 1.1/4\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,26.375186409081788,{"$f":"F293*(1-Elteq!$F$5)","v":26.375186409081788}]
["ANAMET-M",7140407,"NPT 1.1/2\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,29.933374642501413,{"$f":"F294*(1-Elteq!$F$5)","v":29.933374642501413}]
["ANAMET-M",7140507,"NPT 2\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,45.095158446524479,{"$f":"F295*(1-Elteq!$F$5)","v":45.095158446524479}]
["ANAMET-M",7149127,"NPT 1/2\"","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,8.8165029595697835,{"$f":"F296*(1-Elteq!$F$5)","v":8.8165029595697835}]
["ANAMET-M",7149167,"NPT 1/2\"","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,10.813919330810567,{"$f":"F297*(1-Elteq!$F$5)","v":10.813919330810567}]
["ANAMET-M",7149207,"NPT 3/4\"","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,16.834039370643254,{"$f":"F298*(1-Elteq!$F$5)","v":16.834039370643254}]
["ANAMET-M",7149267,"NPT 1\"","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,30.174922668790995,{"$f":"F299*(1-Elteq!$F$5)","v":30.174922668790995}]
["ANAMET-M",7149357,"NPT 1.1/4\"","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,43.367161027683608,{"$f":"F300*(1-Elteq!$F$5)","v":43.367161027683608}]
["ANAMET-M",7149407,"NPT 1.1/2\"","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,63.945194805815397,{"$f":"F301*(1-Elteq!$F$5)","v":63.945194805815397}]
["ANAMET-M",7149507,"NPT 2\"","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",1,87.05948285998781,{"$f":"F302*(1-Elteq!$F$5)","v":87.05948285998781}]
["ANAMET-M",7840107,"-","Multiflex fittings for UI / UIG, Conduit connector, IP 40",1,8.9744382075283582,{"$f":"F303*(1-Elteq!$F$5)","v":8.9744382075283582}]
["ANAMET-M",7840127,"-","Multiflex fittings for UI / UIG, Conduit connector, IP 40",1,8.9744382075283582,{"$f":"F304*(1-Elteq!$F$5)","v":8.9744382075283582}]
["ANAMET-M",7840167,"-","Multiflex fittings for UI / UIG, Conduit connector, IP 40",1,11.148370444134605,{"$f":"F305*(1-Elteq!$F$5)","v":11.148370444134605}]
["ANAMET-M",7840207,"-","Multiflex fittings for UI / UIG, Conduit connector, IP 40",1,16.77829751842258,{"$f":"F306*(1-Elteq!$F$5)","v":16.77829751842258}]
["ANAMET-M",7840267,"-","Multiflex fittings for UI / UIG, Conduit connector, IP 40",1,29.77543939454284,{"$f":"F307*(1-Elteq!$F$5)","v":29.77543939454284}]
["ANAMET-M",7840357,"-","Multiflex fittings for UI / UIG, Conduit connector, IP 40",1,37.384202222664712,{"$f":"F308*(1-Elteq!$F$5)","v":37.384202222664712}]
["ANAMET-M",7840407,"-","Multiflex fittings for UI / UIG, Conduit connector, IP 40",1,44.593481776538418,{"$f":"F309*(1-Elteq!$F$5)","v":44.593481776538418}]
["ANAMET-M",7840507,"-","Multiflex fittings for UI / UIG, Conduit connector, IP 40",1,61.650488556064367,{"$f":"F310*(1-Elteq!$F$5)","v":61.650488556064367}]
["ANAMET-M",8120147,"M 20 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,9.8384369169487886,{"$f":"F311*(1-Elteq!$F$5)","v":9.8384369169487886}]
["ANAMET-M",8120157,"M16 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,7.9896654849631341,{"$f":"F312*(1-Elteq!$F$5)","v":7.9896654849631341}]
["ANAMET-M",8120167,"M16 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,7.3672148018322838,{"$f":"F313*(1-Elteq!$F$5)","v":7.3672148018322838}]
["ANAMET-M",8120177,"M20 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,7.7109562238597684,{"$f":"F314*(1-Elteq!$F$5)","v":7.7109562238597684}]
["ANAMET-M",8120207,"M20 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,8.5470840071698628,{"$f":"F315*(1-Elteq!$F$5)","v":8.5470840071698628}]
["ANAMET-M",8120257,"M25 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,12.727722923720341,{"$f":"F316*(1-Elteq!$F$5)","v":12.727722923720341}]
["ANAMET-M",8120327,"M 32 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,22.018031627165843,{"$f":"F317*(1-Elteq!$F$5)","v":22.018031627165843}]
["ANAMET-M",8120407,"M 40 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,31.559178665604374,{"$f":"F318*(1-Elteq!$F$5)","v":31.559178665604374}]
["ANAMET-M",8120507,"M50 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,47.910121983668461,{"$f":"F319*(1-Elteq!$F$5)","v":47.910121983668461}]
["ANAMET-M",8120637,"M63 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,63.908033571001631,{"$f":"F320*(1-Elteq!$F$5)","v":63.908033571001631}]
["ANAMET-M",8123157,"M16 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,9.9313400039832445,{"$f":"F321*(1-Elteq!$F$5)","v":9.9313400039832445}]
["ANAMET-M",8123167,"M16 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,8.2869553634733908,{"$f":"F322*(1-Elteq!$F$5)","v":8.2869553634733908}]
["ANAMET-M",8123207,"M20 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,9.531856729735086,{"$f":"F323*(1-Elteq!$F$5)","v":9.531856729735086}]
["ANAMET-M",8123257,"M25 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,14.17701108145784,{"$f":"F324*(1-Elteq!$F$5)","v":14.17701108145784}]
["ANAMET-M",8123327,"M32 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,21.943709157538283,{"$f":"F325*(1-Elteq!$F$5)","v":21.943709157538283}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8123407,"M40 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,38.74058729336776,{"$f":"F326*(1-Elteq!$F$5)","v":38.74058729336776}]
["ANAMET-M",8123507,"M50 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,56.893850499900267,{"$f":"F327*(1-Elteq!$F$5)","v":56.893850499900267}]
["ANAMET-M",8123637,"M63 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,76.626466186018519,{"$f":"F328*(1-Elteq!$F$5)","v":76.626466186018519}]
["ANAMET-M",8127157,"M16 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,15.031719482174825,{"$f":"F329*(1-Elteq!$F$5)","v":15.031719482174825}]
["ANAMET-M",8127167,"M16 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,14.808752073292133,{"$f":"F330*(1-Elteq!$F$5)","v":14.808752073292133}]
["ANAMET-M",8127177,"M20 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,14.808752073292133,{"$f":"F331*(1-Elteq!$F$5)","v":14.808752073292133}]
["ANAMET-M",8127207,"M20 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,17.521522214698219,{"$f":"F332*(1-Elteq!$F$5)","v":17.521522214698219}]
["ANAMET-M",8127257,"M25 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,23.170029906393086,{"$f":"F333*(1-Elteq!$F$5)","v":23.170029906393086}]
["ANAMET-M",8127327,"M32 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,59.086363353913406,{"$f":"F334*(1-Elteq!$F$5)","v":59.086363353913406}]
["ANAMET-M",8127407,"M40 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,77.917819095797455,{"$f":"F335*(1-Elteq!$F$5)","v":77.917819095797455}]
["ANAMET-M",8127507,"M50 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,112.04112296355278,{"$f":"F336*(1-Elteq!$F$5)","v":112.04112296355278}]
["ANAMET-M",8127637,"M63 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,168.67484481975657,{"$f":"F337*(1-Elteq!$F$5)","v":168.67484481975657}]
["ANAMET-M",8100097,"PG 9","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,8.2497941286596088,{"$f":"F338*(1-Elteq!$F$5)","v":8.2497941286596088}]
["ANAMET-M",8100107,"PG 9","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,7.6552143716390955,{"$f":"F339*(1-Elteq!$F$5)","v":7.6552143716390955}]
["ANAMET-M",8100117,"PG 11","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,7.7852786934873333,{"$f":"F340*(1-Elteq!$F$5)","v":7.7852786934873333}]
["ANAMET-M",8100127,"PG 11","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,9.2903087034455041,{"$f":"F341*(1-Elteq!$F$5)","v":9.2903087034455041}]
["ANAMET-M",8100137,"PG 13,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,7.7852786934873333,{"$f":"F342*(1-Elteq!$F$5)","v":7.7852786934873333}]
["ANAMET-M",8100167,"PG 16","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,9.4761148775144139,{"$f":"F343*(1-Elteq!$F$5)","v":9.4761148775144139}]
["ANAMET-M",8100217,"PG 21","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,13.192238358892617,{"$f":"F344*(1-Elteq!$F$5)","v":13.192238358892617}]
["ANAMET-M",8100297,"PG 29","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,23.318674845648218,{"$f":"F345*(1-Elteq!$F$5)","v":23.318674845648218}]
["ANAMET-M",8100367,"PG 36","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,31.559178665604374,{"$f":"F346*(1-Elteq!$F$5)","v":31.559178665604374}]
["ANAMET-M",8100427,"PG 42","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,47.910121983668461,{"$f":"F347*(1-Elteq!$F$5)","v":47.910121983668461}]
["ANAMET-M",8100487,"PG 48","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,63.908033571001631,{"$f":"F348*(1-Elteq!$F$5)","v":63.908033571001631}]
["ANAMET-M",8103117,"PG 11","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,8.5470840071698628,{"$f":"F349*(1-Elteq!$F$5)","v":8.5470840071698628}]
["ANAMET-M",8103127,"PG 11","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,10.200758956383165,{"$f":"F350*(1-Elteq!$F$5)","v":10.200758956383165}]
["ANAMET-M",8103137,"PG 13,5","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,9.3832117904799599,{"$f":"F351*(1-Elteq!$F$5)","v":9.3832117904799599}]
["ANAMET-M",8103167,"PG 16","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,9.8477272256522355,{"$f":"F352*(1-Elteq!$F$5)","v":9.8477272256522355}]
["ANAMET-M",8103217,"PG 21","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,14.678687751443896,{"$f":"F353*(1-Elteq!$F$5)","v":14.678687751443896}]
["ANAMET-M",8103297,"PG 29","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,22.761256323441486,{"$f":"F354*(1-Elteq!$F$5)","v":22.761256323441486}]
["ANAMET-M",8103367,"PG 36","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,38.74058729336776,{"$f":"F355*(1-Elteq!$F$5)","v":38.74058729336776}]
["ANAMET-M",8103427,"PG 42","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,60.312684102768216,{"$f":"F356*(1-Elteq!$F$5)","v":60.312684102768216}]
["ANAMET-M",8103487,"PG 48","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,76.626466186018519,{"$f":"F357*(1-Elteq!$F$5)","v":76.626466186018519}]
["ANAMET-M",8107097,"PG 9","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,16.592491344353668,{"$f":"F358*(1-Elteq!$F$5)","v":16.592491344353668}]
["ANAMET-M",8107117,"PG 11","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,14.808752073292133,{"$f":"F359*(1-Elteq!$F$5)","v":14.808752073292133}]
["ANAMET-M",8107127,"PG 9","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,14.808752073292133,{"$f":"F360*(1-Elteq!$F$5)","v":14.808752073292133}]
["ANAMET-M",8107157,"PG 13,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,17.521522214698219,{"$f":"F361*(1-Elteq!$F$5)","v":17.521522214698219}]
["ANAMET-M",8107167,"PG 16","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,21.18190384385575,{"$f":"F362*(1-Elteq!$F$5)","v":21.18190384385575}]
["ANAMET-M",8107217,"PG 21","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,33.203563306114233,{"$f":"F363*(1-Elteq!$F$5)","v":33.203563306114233}]
["ANAMET-M",8107297,"PG 29","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,51.11527848635717,{"$f":"F364*(1-Elteq!$F$5)","v":51.11527848635717}]
["ANAMET-M",8126157,"M16 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,23.746029046006708,{"$f":"F365*(1-Elteq!$F$5)","v":23.746029046006708}]
["ANAMET-M",8126167,"M16 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,22.092354096793411,{"$f":"F366*(1-Elteq!$F$5)","v":22.092354096793411}]
["ANAMET-M",8126177,"M20 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,22.092354096793411,{"$f":"F367*(1-Elteq!$F$5)","v":22.092354096793411}]
["ANAMET-M",8126207,"M20 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,26.0314449870543,{"$f":"F368*(1-Elteq!$F$5)","v":26.0314449870543}]
["ANAMET-M",8126227,"M25 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,32.135177805217999,{"$f":"F369*(1-Elteq!$F$5)","v":32.135177805217999}]
["ANAMET-M",8126287,"M32 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,45.856963760207009,{"$f":"F370*(1-Elteq!$F$5)","v":45.856963760207009}]
["ANAMET-M",8126357,"M40 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,72.213569551881903,{"$f":"F371*(1-Elteq!$F$5)","v":72.213569551881903}]
["ANAMET-M",8140117,"NPT 1/2\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,9.5039858036247509,{"$f":"F372*(1-Elteq!$F$5)","v":9.5039858036247509}]
["ANAMET-M",8140127,"NPT 1/2\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,8.166181350328598,{"$f":"F373*(1-Elteq!$F$5)","v":8.166181350328598}]
["ANAMET-M",8140167,"NPT 1/2\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,9.2903087034455041,{"$f":"F374*(1-Elteq!$F$5)","v":9.2903087034455041}]
["ANAMET-M",8140207,"NPT 3/4\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,12.727722923720341,{"$f":"F375*(1-Elteq!$F$5)","v":12.727722923720341}]
["ANAMET-M",8140267,"NPT 1 \"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,21.646419279028024,{"$f":"F376*(1-Elteq!$F$5)","v":21.646419279028024}]
["ANAMET-M",8140357,"NPT 1.1/4 \"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,32.330274287990349,{"$f":"F377*(1-Elteq!$F$5)","v":32.330274287990349}]
["ANAMET-M",8140407,"NPT 1.1/2\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,50.845859533957245,{"$f":"F378*(1-Elteq!$F$5)","v":50.845859533957245}]
["ANAMET-M",8140507,"NPT 2\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",1,69.630863732324059,{"$f":"F379*(1-Elteq!$F$5)","v":69.630863732324059}]
["ANAMET-M","8107117-3","PG 11","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,35.749107890858298,{"$f":"F380*(1-Elteq!$F$5)","v":35.749107890858298}]
["ANAMET-M","8107157-3","PG 13,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,36.585235674168395,{"$f":"F381*(1-Elteq!$F$5)","v":36.585235674168395}]
["ANAMET-M","8107167-3","PG 16","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,47.937992909778806,{"$f":"F382*(1-Elteq!$F$5)","v":47.937992909778806}]
["ANAMET-M","8107217-3","PG 21","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,49.573087241585213,{"$f":"F383*(1-Elteq!$F$5)","v":49.573087241585213}]
["ANAMET-M","8127157-3","M16 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,37.402782840071602,{"$f":"F384*(1-Elteq!$F$5)","v":37.402782840071602}]
["ANAMET-M","8127167-3","M16 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,35.749107890858298,{"$f":"F385*(1-Elteq!$F$5)","v":35.749107890858298}]
["ANAMET-M","8127207-3","M20 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,36.585235674168395,{"$f":"F386*(1-Elteq!$F$5)","v":36.585235674168395}]
["ANAMET-M","8127227-3","M25 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,47.733606118303008,{"$f":"F387*(1-Elteq!$F$5)","v":47.733606118303008}]
["ANAMET-M",7120168,"M16 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,20.8660333479386,{"$f":"F388*(1-Elteq!$F$5)","v":20.8660333479386}]
["ANAMET-M",7120178,"M20 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,27.099830487950538,{"$f":"F389*(1-Elteq!$F$5)","v":27.099830487950538}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},7120208,"M20 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,27.935958271260631,{"$f":"F390*(1-Elteq!$F$5)","v":27.935958271260631}]
["ANAMET-M",7120258,"M25 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,34.402013128858705,{"$f":"F391*(1-Elteq!$F$5)","v":34.402013128858705}]
["ANAMET-M",7120328,"M32 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,45.54109326428987,{"$f":"F392*(1-Elteq!$F$5)","v":45.54109326428987}]
["ANAMET-M",7120408,"M40 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,63.415647209719012,{"$f":"F393*(1-Elteq!$F$5)","v":63.415647209719012}]
["ANAMET-M",7120508,"M50 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,86.474193411670754,{"$f":"F394*(1-Elteq!$F$5)","v":86.474193411670754}]
["ANAMET-M",7120638,"M63 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,121.84239864568779,{"$f":"F395*(1-Elteq!$F$5)","v":121.84239864568779}]
["ANAMET-M",7129168,"M16 x 1,5","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,39.019296554471119,{"$f":"F396*(1-Elteq!$F$5)","v":39.019296554471119}]
["ANAMET-M",7129178,"M20 x 1,5","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,40.134133598884581,{"$f":"F397*(1-Elteq!$F$5)","v":40.134133598884581}]
["ANAMET-M",7129208,"M20 x 1,5","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,44.760707333200443,{"$f":"F398*(1-Elteq!$F$5)","v":44.760707333200443}]
["ANAMET-M",7129258,"M25 x 1,5","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,58.417461127265334,{"$f":"F399*(1-Elteq!$F$5)","v":58.417461127265334}]
["ANAMET-M",7129328,"M32 x 1,5","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,88.963996144194155,{"$f":"F400*(1-Elteq!$F$5)","v":88.963996144194155}]
["ANAMET-M",7129408,"M40 x 1,5","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,112.15260666799412,{"$f":"F401*(1-Elteq!$F$5)","v":112.15260666799412}]
["ANAMET-M",7129508,"M50 x 1,5","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,165.21884998207483,{"$f":"F402*(1-Elteq!$F$5)","v":165.21884998207483}]
["ANAMET-M",7129638,"M63 x 1,5","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,229.43346374029019,{"$f":"F403*(1-Elteq!$F$5)","v":229.43346374029019}]
["ANAMET-M",7140128,"NPT 1/2\"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,20.8660333479386,{"$f":"F404*(1-Elteq!$F$5)","v":20.8660333479386}]
["ANAMET-M",7140168,"NPT 1/2\"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,27.935958271260631,{"$f":"F405*(1-Elteq!$F$5)","v":27.935958271260631}]
["ANAMET-M",7140208,"NPT 3/4\"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,34.402013128858705,{"$f":"F406*(1-Elteq!$F$5)","v":34.402013128858705}]
["ANAMET-M",7140268,"NPT 1\"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,45.54109326428987,{"$f":"F407*(1-Elteq!$F$5)","v":45.54109326428987}]
["ANAMET-M",7140358,"NPT 1.1/4\"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,63.415647209719012,{"$f":"F408*(1-Elteq!$F$5)","v":63.415647209719012}]
["ANAMET-M",7140408,"NPT 1.1/2\"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,86.474193411670754,{"$f":"F409*(1-Elteq!$F$5)","v":86.474193411670754}]
["ANAMET-M",7140508,"NPT 2\"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,121.84239864568779,{"$f":"F410*(1-Elteq!$F$5)","v":121.84239864568779}]
["ANAMET-M",8143117,"NPT 1/2\"","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,10.200758956383165,{"$f":"F411*(1-Elteq!$F$5)","v":10.200758956383165}]
["ANAMET-M",8143127,"NPT 1/2\"","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,8.5470840071698628,{"$f":"F412*(1-Elteq!$F$5)","v":8.5470840071698628}]
["ANAMET-M",8143167,"NPT 1/2\"","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,9.8105659908384535,{"$f":"F413*(1-Elteq!$F$5)","v":9.8105659908384535}]
["ANAMET-M",8143207,"NPT 3/4\"","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,14.604365281816333,{"$f":"F414*(1-Elteq!$F$5)","v":14.604365281816333}]
["ANAMET-M",8143267,"NPT 1 \"","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,22.538288914558795,{"$f":"F415*(1-Elteq!$F$5)","v":22.538288914558795}]
["ANAMET-M",8143357,"NPT 1.1/4 \"","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,38.982135319657331,{"$f":"F416*(1-Elteq!$F$5)","v":38.982135319657331}]
["ANAMET-M",8143407,"NPT 1.1/2\"","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,61.334618060147214,{"$f":"F417*(1-Elteq!$F$5)","v":61.334618060147214}]
["ANAMET-M",8143507,"NPT 2\"","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",1,83.956519753037028,{"$f":"F418*(1-Elteq!$F$5)","v":83.956519753037028}]
["ANAMET-M",8147097,"NPT 3/8\"","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,16.462427022505434,{"$f":"F419*(1-Elteq!$F$5)","v":16.462427022505434}]
["ANAMET-M",8147107,"NPT 3/8\"","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,14.808752073292133,{"$f":"F420*(1-Elteq!$F$5)","v":14.808752073292133}]
["ANAMET-M",8147127,"NPT 1/2\"","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,14.808752073292133,{"$f":"F421*(1-Elteq!$F$5)","v":14.808752073292133}]
["ANAMET-M",8147157,"NPT 1/2\"","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,21.18190384385575,{"$f":"F422*(1-Elteq!$F$5)","v":21.18190384385575}]
["ANAMET-M",8147217,"NPT 3/4\"","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",1,33.203563306114233,{"$f":"F423*(1-Elteq!$F$5)","v":33.203563306114233}]
["ANAMET-M",7149128,"NPT 1/2\"","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,39.019296554471119,{"$f":"F424*(1-Elteq!$F$5)","v":39.019296554471119}]
["ANAMET-M",7149168,"NPT 1/2\"","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,44.760707333200443,{"$f":"F425*(1-Elteq!$F$5)","v":44.760707333200443}]
["ANAMET-M",7149208,"NPT 3/4\"","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,58.417461127265334,{"$f":"F426*(1-Elteq!$F$5)","v":58.417461127265334}]
["ANAMET-M",7149268,"NPT 1 \"","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,88.963996144194155,{"$f":"F427*(1-Elteq!$F$5)","v":88.963996144194155}]
["ANAMET-M",7149358,"NPT 1.1/4 \"","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,112.15260666799412,{"$f":"F428*(1-Elteq!$F$5)","v":112.15260666799412}]
["ANAMET-M",7149408,"NPT 1.1/2\"","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,165.21884998207483,{"$f":"F429*(1-Elteq!$F$5)","v":165.21884998207483}]
["ANAMET-M",7149508,"NPT 2\"","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,229.43346374029019,{"$f":"F430*(1-Elteq!$F$5)","v":229.43346374029019}]
["ANAMET-M",8100118,"PG 11","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,24.052609233220409,{"$f":"F431*(1-Elteq!$F$5)","v":24.052609233220409}]
["ANAMET-M",8100128,"PG 11","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,25.706284182433713,{"$f":"F432*(1-Elteq!$F$5)","v":25.706284182433713}]
["ANAMET-M",8100168,"PG 16","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,33.59375627165894,{"$f":"F433*(1-Elteq!$F$5)","v":33.59375627165894}]
["ANAMET-M",8100218,"PG 21","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,39.929746807408776,{"$f":"F434*(1-Elteq!$F$5)","v":39.929746807408776}]
["ANAMET-M",8109118,"PG 11","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,39.548844150567511,{"$f":"F435*(1-Elteq!$F$5)","v":39.548844150567511}]
["ANAMET-M",8109128,"PG 11","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,41.202519099780815,{"$f":"F436*(1-Elteq!$F$5)","v":41.202519099780815}]
["ANAMET-M",8109168,"PG 16","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,55.435272033459327,{"$f":"F437*(1-Elteq!$F$5)","v":55.435272033459327}]
["ANAMET-M",8109218,"PG 21","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,65.032160924118529,{"$f":"F438*(1-Elteq!$F$5)","v":65.032160924118529}]
["ANAMET-M",8120148,"M20 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,25.706284182433713,{"$f":"F439*(1-Elteq!$F$5)","v":25.706284182433713}]
["ANAMET-M",8120158,"M16 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,25.706284182433713,{"$f":"F440*(1-Elteq!$F$5)","v":25.706284182433713}]
["ANAMET-M",8120168,"M16 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,24.052609233220409,{"$f":"F441*(1-Elteq!$F$5)","v":24.052609233220409}]
["ANAMET-M",8120178,"M20 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,32.757628488348843,{"$f":"F442*(1-Elteq!$F$5)","v":32.757628488348843}]
["ANAMET-M",8120208,"M20 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,33.59375627165894,{"$f":"F443*(1-Elteq!$F$5)","v":33.59375627165894}]
["ANAMET-M",8120258,"M25 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,39.929746807408776,{"$f":"F444*(1-Elteq!$F$5)","v":39.929746807408776}]
["ANAMET-M",8120328,"M 32 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,52.945469300935933,{"$f":"F445*(1-Elteq!$F$5)","v":52.945469300935933}]
["ANAMET-M",8120408,"M40 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,98.728110591515374,{"$f":"F446*(1-Elteq!$F$5)","v":98.728110591515374}]
["ANAMET-M",8127158,"M16 x 1,5","Stainless steel 316 fittings for UI, Straight cablehose male thread, IP 68",1,48.681217606054439,{"$f":"F447*(1-Elteq!$F$5)","v":48.681217606054439}]
["ANAMET-M",8127168,"M16 x 1,5","Stainless steel 316 fittings for UI, Straight cablehose male thread, IP 68",1,47.027542656841142,{"$f":"F448*(1-Elteq!$F$5)","v":47.027542656841142}]
["ANAMET-M",8127178,"M20 x 1,5","Stainless steel 316 fittings for UI, Straight cablehose male thread, IP 68",1,50.167666998605718,{"$f":"F449*(1-Elteq!$F$5)","v":50.167666998605718}]
["ANAMET-M",8127208,"M20 x 1,5","Stainless steel 316 fittings for UI, Straight cablehose male thread, IP 68",1,56.122754877514289,{"$f":"F450*(1-Elteq!$F$5)","v":56.122754877514289}]
["ANAMET-M",8140118,"NPT 1/2\"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,26.709637522405824,{"$f":"F451*(1-Elteq!$F$5)","v":26.709637522405824}]
["ANAMET-M",8140128,"NPT 1/2\"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,25.055962573192524,{"$f":"F452*(1-Elteq!$F$5)","v":25.055962573192524}]
["ANAMET-M",8140168,"NPT 1/2\"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,35.024463811989548,{"$f":"F453*(1-Elteq!$F$5)","v":35.024463811989548}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8140208,"NPT 3/4\"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,41.56484113921519,{"$f":"F454*(1-Elteq!$F$5)","v":41.56484113921519}]
["ANAMET-M",8140268,"NPT 1 \"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",1,49.96328020712992,{"$f":"F455*(1-Elteq!$F$5)","v":49.96328020712992}]
["ANAMET-M",8149118,"NPT 1/2\"","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,42.874774666400995,{"$f":"F456*(1-Elteq!$F$5)","v":42.874774666400995}]
["ANAMET-M",8149128,"NPT 1/2\"","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,41.221099717187698,{"$f":"F457*(1-Elteq!$F$5)","v":41.221099717187698}]
["ANAMET-M",8149168,"NPT 1/2\"","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,57.813591061541366,{"$f":"F458*(1-Elteq!$F$5)","v":57.813591061541366}]
["ANAMET-M",8149208,"NPT 3/4\"","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",1,67.744931065524611,{"$f":"F459*(1-Elteq!$F$5)","v":67.744931065524611}]
["ANAMET-M",7121168,"M16 x 1,5","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",1,26.300863939454221,{"$f":"F460*(1-Elteq!$F$5)","v":26.300863939454221}]
["ANAMET-M",7121178,"M20 x 1,5","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",1,34.392722820155257,{"$f":"F461*(1-Elteq!$F$5)","v":34.392722820155257}]
["ANAMET-M",7121208,"M20 x 1,5","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",1,35.228850603465354,{"$f":"F462*(1-Elteq!$F$5)","v":35.228850603465354}]
["ANAMET-M",7121258,"M25 x 1,5","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",1,43.088451766580249,{"$f":"F463*(1-Elteq!$F$5)","v":43.088451766580249}]
["ANAMET-M",7121328,"M32 x 1,5","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",1,56.364302903803875,{"$f":"F464*(1-Elteq!$F$5)","v":56.364302903803875}]
["ANAMET-M",7121408,"M40 x 1,5","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",1,79.385687870941837,{"$f":"F465*(1-Elteq!$F$5)","v":79.385687870941837}]
["ANAMET-M",7121508,"M50 x 1,5","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",1,122.90149383788057,{"$f":"F466*(1-Elteq!$F$5)","v":122.90149383788057}]
["ANAMET-M",7121638,"M63 x 1,5","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",1,167.8015558016327,{"$f":"F467*(1-Elteq!$F$5)","v":167.8015558016327}]
["ANAMET-M",7141128,"NPT 1/2\"","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",1,26.300863939454221,{"$f":"F468*(1-Elteq!$F$5)","v":26.300863939454221}]
["ANAMET-M",7141168,"NPT 1/2\"","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",1,35.228850603465354,{"$f":"F469*(1-Elteq!$F$5)","v":35.228850603465354}]
["ANAMET-M",7141208,"NPT 3/4\"","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",1,43.088451766580249,{"$f":"F470*(1-Elteq!$F$5)","v":43.088451766580249}]
["ANAMET-M",7141268,"NPT 1 \"","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",1,56.364302903803875,{"$f":"F471*(1-Elteq!$F$5)","v":56.364302903803875}]
["ANAMET-M",7141358,"NPT 1.1/4 \"","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",1,79.385687870941837,{"$f":"F472*(1-Elteq!$F$5)","v":79.385687870941837}]
["ANAMET-M",7141408,"NPT 1.1/2\"","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",1,122.90149383788057,{"$f":"F473*(1-Elteq!$F$5)","v":122.90149383788057}]
["ANAMET-M",7141508,"NPT 2\"","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",1,167.8015558016327,{"$f":"F474*(1-Elteq!$F$5)","v":167.8015558016327}]
["ANAMET-M",8100072,"PG 7","Multiflex fittings for UI - CAP, Straight fixed with male thread, IP 40",1,5.2397341087432645,{"$f":"F475*(1-Elteq!$F$5)","v":5.2397341087432645}]
["ANAMET-M",8100092,"PG 9","Multiflex fittings for UI - CAP, Straight fixed with male thread, IP 40",1,5.2397341087432645,{"$f":"F476*(1-Elteq!$F$5)","v":5.2397341087432645}]
["ANAMET-M",8120112,"M12 x 1,5","Multiflex fittings for UI - CAP, Straight fixed with male thread, IP 40",1,5.4069596654052834,{"$f":"F477*(1-Elteq!$F$5)","v":5.4069596654052834}]
["ANAMET-M",8120122,"M12 x 1,5","Multiflex fittings for UI - CAP, Straight fixed with male thread, IP 40",1,5.2397341087432645,{"$f":"F478*(1-Elteq!$F$5)","v":5.2397341087432645}]
["ANAMET-M",8120132,"M16 x 1,5","Multiflex fittings for UI - CAP, Straight fixed with male thread, IP 40",1,5.2397341087432645,{"$f":"F479*(1-Elteq!$F$5)","v":5.2397341087432645}]
["ANAMET-M",8120142,"M20 x 1,5","Multiflex fittings for UI - CAP, Straight fixed with male thread, IP 40",1,5.4069596654052834,{"$f":"F480*(1-Elteq!$F$5)","v":5.4069596654052834}]
["ANAMET-M",8120152,"M16 x 1,5","Multiflex fittings for UI - CAP, Straight fixed with male thread, IP 40",1,4.9796054650467907,{"$f":"F481*(1-Elteq!$F$5)","v":4.9796054650467907}]
["ANAMET-M",8172069,"-","Multiflex fittings for  UI-CAP, Connection ring for UI-CAP",1,0.89186963553076837,{"$f":"F482*(1-Elteq!$F$5)","v":0.89186963553076837}]
["ANAMET-M",8172099,"-","Multiflex fittings for  UI-CAP, Connection ring for UI-CAP",1,3.0100600199163439,{"$f":"F483*(1-Elteq!$F$5)","v":3.0100600199163439}]
["ANAMET-M",432310,"PG 7","Multiflex fittings for  UI-CAP, Straight fixed with male thread, IP 40",1,6.1130231268671418,{"$f":"F484*(1-Elteq!$F$5)","v":6.1130231268671418}]
["ANAMET-M",555810,"M 12 x 1,5","Multiflex fittings for  UI-CAP, Straight fixed with male thread, IP 40",1,6.8005059709221083,{"$f":"F485*(1-Elteq!$F$5)","v":6.8005059709221083}]
["ANAMET-M",559730,"M 12 x 1,5","Multiflex fittings for  UI-CAP, Straight swivel with male thread, IP 40",1,17.967457032463603,{"$f":"F486*(1-Elteq!$F$5)","v":17.967457032463603}]
["ANAMET-M",559830,"M 16 x 1,5","Multiflex fittings for  UI-CAP, Straight swivel with male thread, IP 40",1,17.967457032463603,{"$f":"F487*(1-Elteq!$F$5)","v":17.967457032463603}]
["ANAMET-M",572610,"M 12 x 1,5","Multiflex fittings for  UI-CAP, Straight fixed with male thread, IP 40",1,6.1873455964947048,{"$f":"F488*(1-Elteq!$F$5)","v":6.1873455964947048}]
["ANAMET-M",594010,"-","Multiflex fittings for  UI-CAP, Connection ring for UI-CAP",1,2.0438679147580112,{"$f":"F489*(1-Elteq!$F$5)","v":2.0438679147580112}]
["ANAMET-M",2227031,"-","Multiflex fittings for  UI-CAP, Connection ring for UI-CAP",1,1.1891595140410245,{"$f":"F490*(1-Elteq!$F$5)","v":1.1891595140410245}]
["ANAMET-M",2960120,"NPT 1/2\"","Multiflex fittings for  RWA, Straight fixed with male thread, IP 40",1,1.5607718621788444,{"$f":"F491*(1-Elteq!$F$5)","v":1.5607718621788444}]
["ANAMET-M",2960160,"NPT 1/2\"","Multiflex fittings for  RWA, Straight fixed with male thread, IP 40",1,1.8952229755028829,{"$f":"F492*(1-Elteq!$F$5)","v":1.8952229755028829}]
["ANAMET-M",2960200,"NPT 3/4\"","Multiflex fittings for  RWA, Straight fixed with male thread, IP 40",1,2.1367710017924657,{"$f":"F493*(1-Elteq!$F$5)","v":2.1367710017924657}]
["ANAMET-M",2960260,"NPT 1\"","Multiflex fittings for  RWA, Straight fixed with male thread, IP 40",1,6.939860601473792,{"$f":"F494*(1-Elteq!$F$5)","v":6.939860601473792}]
["ANAMET-M",2960350,"NPT 1 1/4\"","Multiflex fittings for  RWA, Straight fixed with male thread, IP 40",1,15.236106273650625,{"$f":"F495*(1-Elteq!$F$5)","v":15.236106273650625}]
["ANAMET-M",2960400,"NPT 1 1/2\"","Multiflex fittings for  RWA, Straight fixed with male thread, IP 40",1,21.367710017924658,{"$f":"F496*(1-Elteq!$F$5)","v":21.367710017924658}]
["ANAMET-M",2960500,"NPT 2\"","Multiflex fittings for  RWA, Straight fixed with male thread, IP 40",1,31.865758852818079,{"$f":"F497*(1-Elteq!$F$5)","v":31.865758852818079}]
["ANAMET-M",2961125,"NPT 1/2\"","Multiflex fittings for  RWA, Straight fixed with male thread, IP 40",1,1.0590951921927874,{"$f":"F498*(1-Elteq!$F$5)","v":1.0590951921927874}]
["ANAMET-M",2961165,"NPT 1/2\"","Multiflex fittings for  RWA, Straight fixed with male thread, IP 40",1,1.0590951921927874,{"$f":"F499*(1-Elteq!$F$5)","v":1.0590951921927874}]
["ANAMET-M",2961205,"NPT 3/4\"","Multiflex fittings for  RWA, Straight fixed with male thread, IP 40",1,1.7930295797649822,{"$f":"F500*(1-Elteq!$F$5)","v":1.7930295797649822}]
["ANAMET-M",2962160,"-","Multiflex fittings for  RWA, Conduit isolation bushing for RWA",1,0.35303173073092919,{"$f":"F501*(1-Elteq!$F$5)","v":0.35303173073092919}]
["ANAMET-M",2962200,"-","Multiflex fittings for  RWA, Conduit isolation bushing for RWA",1,0.39948327424815672,{"$f":"F502*(1-Elteq!$F$5)","v":0.39948327424815672}]
["ANAMET-M",2964120,"-","Multiflex fittings for  RWA, Conduit isolation bushing for RWA",1,0.35303173073092919,{"$f":"F503*(1-Elteq!$F$5)","v":0.35303173073092919}]
["ANAMET-M",2969120,"NPT 1/2\"","Multiflex fittings for  RWA, 90° elbow fixed with male thread, IP 40",1,1.9230939016132194,{"$f":"F504*(1-Elteq!$F$5)","v":1.9230939016132194}]
["ANAMET-M",2969160,"NPT 1/2\"","Multiflex fittings for  RWA, 90° elbow fixed with male thread, IP 40",1,3.1772855765783623,{"$f":"F505*(1-Elteq!$F$5)","v":3.1772855765783623}]
["ANAMET-M",2969200,"NPT 3/4\"","Multiflex fittings for  RWA, 90° elbow fixed with male thread, IP 40",1,5.1468310217088087,{"$f":"F506*(1-Elteq!$F$5)","v":5.1468310217088087}]
["ANAMET-M",2969260,"NPT 1\"","Multiflex fittings for  RWA, 90° elbow fixed with male thread, IP 40",1,15.886427882891812,{"$f":"F507*(1-Elteq!$F$5)","v":15.886427882891812}]
["ANAMET-M",2969350,"NPT 1 1/4\"","Multiflex fittings for  RWA, 90° elbow fixed with male thread, IP 40",1,25.919961282612956,{"$f":"F508*(1-Elteq!$F$5)","v":25.919961282612956}]
["ANAMET-M",2969400,"NPT 1 1/2\"","Multiflex fittings for  RWA, 90° elbow fixed with male thread, IP 40",1,66.704416490738723,{"$f":"F509*(1-Elteq!$F$5)","v":66.704416490738723}]
["ANAMET-M",2969500,"NPT 2\"","Multiflex fittings for  RWA, 90° elbow fixed with male thread, IP 40",1,67.819253535152185,{"$f":"F510*(1-Elteq!$F$5)","v":67.819253535152185}]
["ANAMET-M",8834160,"-","Multiflex fittings for  RWA, Conduit connector, IP 40",1,2.5734155108544043,{"$f":"F511*(1-Elteq!$F$5)","v":2.5734155108544043}]
["ANAMET-M",8834200,"-","Multiflex fittings for  RWA, Conduit connector, IP 40",1,4.1434776817366954,{"$f":"F512*(1-Elteq!$F$5)","v":4.1434776817366954}]
["ANAMET-M",8834260,"-","Multiflex fittings for  RWA, Conduit connector, IP 40",1,8.3426972156940646,{"$f":"F513*(1-Elteq!$F$5)","v":8.3426972156940646}]
["ANAMET-M",8834350,"-","Multiflex fittings for  RWA, Conduit connector, IP 40",1,16.44384640509854,{"$f":"F514*(1-Elteq!$F$5)","v":16.44384640509854}]
["ANAMET-M",8834400,"-","Multiflex fittings for  RWA, Conduit connector, IP 40",1,22.296740888269209,{"$f":"F515*(1-Elteq!$F$5)","v":22.296740888269209}]
["ANAMET-M",8420160,"M16 x 1,5","Multiflex fittings for  ANAFLEX, Straight fixed with male thread, IP 69K",1,5.0817988607846907,{"$f":"F516*(1-Elteq!$F$5)","v":5.0817988607846907}]
["ANAMET-M",8420170,"M20 x 1,5","Multiflex fittings for  ANAFLEX, Straight fixed with male thread, IP 69K",1,5.1932825652260366,{"$f":"F517*(1-Elteq!$F$5)","v":5.1932825652260366}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8420200,"M20 x 1,5","Multiflex fittings for  ANAFLEX, Straight fixed with male thread, IP 69K",1,7.0885055407289199,{"$f":"F518*(1-Elteq!$F$5)","v":7.0885055407289199}]
["ANAMET-M",8420250,"M25 x 1,5","Multiflex fittings for  ANAFLEX, Straight fixed with male thread, IP 69K",1,10.098565560645262,{"$f":"F519*(1-Elteq!$F$5)","v":10.098565560645262}]
["ANAMET-M",8440120,"NPT 1/2\"","Multiflex fittings for  ANAFLEX, Straight fixed with male thread, IP 69K",1,5.1932825652260366,{"$f":"F520*(1-Elteq!$F$5)","v":5.1932825652260366}]
["ANAMET-M",8440160,"NPT 1/2\"","Multiflex fittings for  ANAFLEX, Straight fixed with male thread, IP 69K",1,7.2092795538737109,{"$f":"F521*(1-Elteq!$F$5)","v":7.2092795538737109}]
["ANAMET-M",8440180,"NPT 3/4\"","Multiflex fittings for  ANAFLEX, Straight fixed with male thread, IP 69K",1,7.7388271499701045,{"$f":"F522*(1-Elteq!$F$5)","v":7.7388271499701045}]
["ANAMET-M",8440200,"NPT 3/4\"","Multiflex fittings for  ANAFLEX, Straight fixed with male thread, IP 69K",1,10.098565560645262,{"$f":"F523*(1-Elteq!$F$5)","v":10.098565560645262}]
["ANAMET-M",2601100,"M10 X 1,0","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",1,2.0624485321649022,{"$f":"F524*(1-Elteq!$F$5)","v":2.0624485321649022}]
["ANAMET-M",2601110,"M12 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",1,2.3876093367854945,{"$f":"F525*(1-Elteq!$F$5)","v":2.3876093367854945}]
["ANAMET-M",2601120,"M12 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",1,2.3876093367854945,{"$f":"F526*(1-Elteq!$F$5)","v":2.3876093367854945}]
["ANAMET-M",2601150,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",1,2.3876093367854945,{"$f":"F527*(1-Elteq!$F$5)","v":2.3876093367854945}]
["ANAMET-M",2601160,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",1,2.7313507588129782,{"$f":"F528*(1-Elteq!$F$5)","v":2.7313507588129782}]
["ANAMET-M",2601170,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",1,2.9728987851025614,{"$f":"F529*(1-Elteq!$F$5)","v":2.9728987851025614}]
["ANAMET-M",2601180,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",1,3.5581882334196284,{"$f":"F530*(1-Elteq!$F$5)","v":3.5581882334196284}]
["ANAMET-M",2601200,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",1,3.5581882334196284,{"$f":"F531*(1-Elteq!$F$5)","v":3.5581882334196284}]
["ANAMET-M",2601250,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",1,5.1747019478191456,{"$f":"F532*(1-Elteq!$F$5)","v":5.1747019478191456}]
["ANAMET-M",2601320,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",1,9.0115994423421384,{"$f":"F533*(1-Elteq!$F$5)","v":9.0115994423421384}]
["ANAMET-M",2602070,"PG 7","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",1,2.303996558454485,{"$f":"F534*(1-Elteq!$F$5)","v":2.303996558454485}]
["ANAMET-M",2602090,"PG 9","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",1,2.6291573630750777,{"$f":"F535*(1-Elteq!$F$5)","v":2.6291573630750777}]
["ANAMET-M",2602110,"PG 11","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",1,2.8521247719577696,{"$f":"F536*(1-Elteq!$F$5)","v":2.8521247719577696}]
["ANAMET-M",2602130,"PG 13,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",1,3.5117366899024001,{"$f":"F537*(1-Elteq!$F$5)","v":3.5117366899024001}]
["ANAMET-M",2602160,"PG 16","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",1,3.6325107030471924,{"$f":"F538*(1-Elteq!$F$5)","v":3.6325107030471924}]
["ANAMET-M",2602210,"PG 21","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",1,5.2861856522604924,{"$f":"F539*(1-Elteq!$F$5)","v":5.2861856522604924}]
["ANAMET-M",2602290,"PG 29","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",1,9.9685012387970264,{"$f":"F540*(1-Elteq!$F$5)","v":9.9685012387970264}]
["ANAMET-M",2603110,"M12 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 54",1,2.7870926110336511,{"$f":"F541*(1-Elteq!$F$5)","v":2.7870926110336511}]
["ANAMET-M",2603120,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 54",1,2.9636084763991155,{"$f":"F542*(1-Elteq!$F$5)","v":2.9636084763991155}]
["ANAMET-M",2603160,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 54",1,2.9636084763991155,{"$f":"F543*(1-Elteq!$F$5)","v":2.9636084763991155}]
["ANAMET-M",2603170,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 54",1,3.2423177375024812,{"$f":"F544*(1-Elteq!$F$5)","v":3.2423177375024812}]
["ANAMET-M",2603200,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 54",1,3.7997362597092108,{"$f":"F545*(1-Elteq!$F$5)","v":3.7997362597092108}]
["ANAMET-M",2603250,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 54",1,6.2802486835291607,{"$f":"F546*(1-Elteq!$F$5)","v":6.2802486835291607}]
["ANAMET-M",2603320,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 54",1,11.027596430989814,{"$f":"F547*(1-Elteq!$F$5)","v":11.027596430989814}]
["ANAMET-M",2611100,"M10 x 1,0","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",1,3.0658018721370164,{"$f":"F548*(1-Elteq!$F$5)","v":3.0658018721370164}]
["ANAMET-M",2611110,"M12 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",1,3.0658018721370164,{"$f":"F549*(1-Elteq!$F$5)","v":3.0658018721370164}]
["ANAMET-M",2611120,"M12 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",1,3.0658018721370164,{"$f":"F550*(1-Elteq!$F$5)","v":3.0658018721370164}]
["ANAMET-M",2611150,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",1,3.2144468113921443,{"$f":"F551*(1-Elteq!$F$5)","v":3.2144468113921443}]
["ANAMET-M",2611160,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",1,3.2237371200955898,{"$f":"F552*(1-Elteq!$F$5)","v":3.2237371200955898}]
["ANAMET-M",2611170,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",1,3.6696719378609739,{"$f":"F553*(1-Elteq!$F$5)","v":3.6696719378609739}]
["ANAMET-M",2611180,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",1,4.3757353993228323,{"$f":"F554*(1-Elteq!$F$5)","v":4.3757353993228323}]
["ANAMET-M",2611200,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",1,4.4128966341366143,{"$f":"F555*(1-Elteq!$F$5)","v":4.4128966341366143}]
["ANAMET-M",2611250,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",1,6.6239901055566444,{"$f":"F556*(1-Elteq!$F$5)","v":6.6239901055566444}]
["ANAMET-M",2611320,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",1,11.715079275044781,{"$f":"F557*(1-Elteq!$F$5)","v":11.715079275044781}]
["ANAMET-M",2612070,"PG 7","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",1,3.2980595897231542,{"$f":"F558*(1-Elteq!$F$5)","v":3.2980595897231542}]
["ANAMET-M",2612090,"PG 9","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",1,3.3352208245369357,{"$f":"F559*(1-Elteq!$F$5)","v":3.3352208245369357}]
["ANAMET-M",2612110,"PG 11","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",1,3.474575455088619,{"$f":"F560*(1-Elteq!$F$5)","v":3.474575455088619}]
["ANAMET-M",2612130,"PG 13,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",1,4.2178001513642585,{"$f":"F561*(1-Elteq!$F$5)","v":4.2178001513642585}]
["ANAMET-M",2612160,"PG 16","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",1,4.3571547819159422,{"$f":"F562*(1-Elteq!$F$5)","v":4.3571547819159422}]
["ANAMET-M",2612210,"PG 21","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",1,7.3207632583150577,{"$f":"F563*(1-Elteq!$F$5)","v":7.3207632583150577}]
["ANAMET-M",2612290,"PG 29","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",1,12.959980641306478,{"$f":"F564*(1-Elteq!$F$5)","v":12.959980641306478}]
["ANAMET-M",2622100,"- ","Multiflex fittings for FCE / FCD, Straight fixed box connector, IP 54",1,1.6165137143995176,{"$f":"F565*(1-Elteq!$F$5)","v":1.6165137143995176}]
["ANAMET-M",2622120,"- ","Multiflex fittings for FCE / FCD, Straight fixed box connector, IP 54",1,1.7465780362477545,{"$f":"F566*(1-Elteq!$F$5)","v":1.7465780362477545}]
["ANAMET-M",2622160,"- ","Multiflex fittings for FCE / FCD, Straight fixed box connector, IP 54",1,2.2482547062338121,{"$f":"F567*(1-Elteq!$F$5)","v":2.2482547062338121}]
["ANAMET-M",2622180,"- ","Multiflex fittings for FCE / FCD, Straight fixed box connector, IP 54",1,2.2947062497510395,{"$f":"F568*(1-Elteq!$F$5)","v":2.2947062497510395}]
["ANAMET-M",2622200,"- ","Multiflex fittings for FCE / FCD, Straight fixed box connector, IP 54",1,2.4061899541923855,{"$f":"F569*(1-Elteq!$F$5)","v":2.4061899541923855}]
["ANAMET-M",2622250,"- ","Multiflex fittings for FCE / FCD, Straight fixed box connector, IP 54",1,3.3816723680541636,{"$f":"F570*(1-Elteq!$F$5)","v":3.3816723680541636}]
["ANAMET-M",2622320,"- ","Multiflex fittings for FCE / FCD, Straight fixed box connector, IP 54",1,5.0725085520812456,{"$f":"F571*(1-Elteq!$F$5)","v":5.0725085520812456}]
["ANAMET-M",2641100,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",1,1.4585784664409442,{"$f":"F572*(1-Elteq!$F$5)","v":1.4585784664409442}]
["ANAMET-M",2641120,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",1,1.5236106273650625,{"$f":"F573*(1-Elteq!$F$5)","v":1.5236106273650625}]
["ANAMET-M",2641160,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",1,1.9045132842063281,{"$f":"F574*(1-Elteq!$F$5)","v":1.9045132842063281}]
["ANAMET-M",2641180,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",1,1.9045132842063281,{"$f":"F575*(1-Elteq!$F$5)","v":1.9045132842063281}]
["ANAMET-M",2641200,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",1,2.3597384106751584,{"$f":"F576*(1-Elteq!$F$5)","v":2.3597384106751584}]
["ANAMET-M",2641250,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",1,3.2887692810197087,{"$f":"F577*(1-Elteq!$F$5)","v":3.2887692810197087}]
["ANAMET-M",2641320,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",1,4.8959926867157808,{"$f":"F578*(1-Elteq!$F$5)","v":4.8959926867157808}]
["ANAMET-M",7120144,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",1,4.7752186735709889,{"$f":"F579*(1-Elteq!$F$5)","v":4.7752186735709889}]
["ANAMET-M",7120154,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",1,4.4686384863572872,{"$f":"F580*(1-Elteq!$F$5)","v":4.4686384863572872}]
["ANAMET-M",7120164,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",1,3.3538014419438267,{"$f":"F581*(1-Elteq!$F$5)","v":3.3538014419438267}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},7120174,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",1,3.6603816291575288,{"$f":"F582*(1-Elteq!$F$5)","v":3.6603816291575288}]
["ANAMET-M",7120204,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",1,3.8647684206333297,{"$f":"F583*(1-Elteq!$F$5)","v":3.8647684206333297}]
["ANAMET-M",7120254,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",1,6.0015394224257959,{"$f":"F584*(1-Elteq!$F$5)","v":6.0015394224257959}]
["ANAMET-M",7120324,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",1,9.5504373471419779,{"$f":"F585*(1-Elteq!$F$5)","v":9.5504373471419779}]
["ANAMET-M",7120404,"M40 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",1,17.744489623580915,{"$f":"F586*(1-Elteq!$F$5)","v":17.744489623580915}]
["ANAMET-M",7129144,"M20 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",1,8.20334258514238,{"$f":"F587*(1-Elteq!$F$5)","v":8.20334258514238}]
["ANAMET-M",7129154,"M16 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",1,7.1442473929495938,{"$f":"F588*(1-Elteq!$F$5)","v":7.1442473929495938}]
["ANAMET-M",7129164,"M16 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",1,6.0294103485361328,{"$f":"F589*(1-Elteq!$F$5)","v":6.0294103485361328}]
["ANAMET-M",7129174,"M20 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",1,7.0885055407289199,{"$f":"F590*(1-Elteq!$F$5)","v":7.0885055407289199}]
["ANAMET-M",7129204,"M20 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",1,7.1906989364668199,{"$f":"F591*(1-Elteq!$F$5)","v":7.1906989364668199}]
["ANAMET-M",7129254,"M25 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",1,11.371337853017296,{"$f":"F592*(1-Elteq!$F$5)","v":11.371337853017296}]
["ANAMET-M",7129324,"M32 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",1,20.698807791276582,{"$f":"F593*(1-Elteq!$F$5)","v":20.698807791276582}]
["ANAMET-M",7830160,"M 16 x 1,5","Multiflex fittings for FCE / FCD, Elbow fitting male/female",1,3.6046397769368554,{"$f":"F594*(1-Elteq!$F$5)","v":3.6046397769368554}]
["ANAMET-M",7830200,"M 20 x 1,5","Multiflex fittings for FCE / FCD, Elbow fitting male/female",1,4.1434776817366954,{"$f":"F595*(1-Elteq!$F$5)","v":4.1434776817366954}]
["ANAMET-M",7830250,"M 25 x 1,5","Multiflex fittings for FCE / FCD, Elbow fitting male/female",1,8.5377936984664178,{"$f":"F596*(1-Elteq!$F$5)","v":8.5377936984664178}]
["ANAMET-M",7830320,"M 32 x 1,5","Multiflex fittings for FCE / FCD, Elbow fitting male/female",1,14.334946329416413,{"$f":"F597*(1-Elteq!$F$5)","v":14.334946329416413}]
["ANAMET-M",8130154,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 65",1,8.6214064767974268,{"$f":"F598*(1-Elteq!$F$5)","v":8.6214064767974268}]
["ANAMET-M",8130164,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 65",1,7.8688914718183423,{"$f":"F599*(1-Elteq!$F$5)","v":7.8688914718183423}]
["ANAMET-M",8130204,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 65",1,8.9372769727145744,{"$f":"F600*(1-Elteq!$F$5)","v":8.9372769727145744}]
["ANAMET-M",8130254,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 65",1,11.770821127265453,{"$f":"F601*(1-Elteq!$F$5)","v":11.770821127265453}]
["ANAMET-M",8130324,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 65",1,19.583970746863123,{"$f":"F602*(1-Elteq!$F$5)","v":19.583970746863123}]
["ANAMET-M",7100114,"PG 11","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",1,3.4095432941644996,{"$f":"F603*(1-Elteq!$F$5)","v":3.4095432941644996}]
["ANAMET-M",7100134,"PG 13,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",1,3.4188336028679456,{"$f":"F604*(1-Elteq!$F$5)","v":3.4188336028679456}]
["ANAMET-M",7100164,"PG 16","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",1,4.0319939772953486,{"$f":"F605*(1-Elteq!$F$5)","v":4.0319939772953486}]
["ANAMET-M",7100214,"PG 21","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",1,6.1223134355705868,{"$f":"F606*(1-Elteq!$F$5)","v":6.1223134355705868}]
["ANAMET-M",7100294,"PG 29","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",1,9.9685012387970264,{"$f":"F607*(1-Elteq!$F$5)","v":9.9685012387970264}]
["ANAMET-M",7109114,"PG 11","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",1,6.2802486835291607,{"$f":"F608*(1-Elteq!$F$5)","v":6.2802486835291607}]
["ANAMET-M",7109134,"PG 13,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",1,6.4753451663015156,{"$f":"F609*(1-Elteq!$F$5)","v":6.4753451663015156}]
["ANAMET-M",7109164,"PG 16","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",1,7.6737949890459864,{"$f":"F610*(1-Elteq!$F$5)","v":7.6737949890459864}]
["ANAMET-M",7109214,"PG 21","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",1,11.24127353116906,{"$f":"F611*(1-Elteq!$F$5)","v":11.24127353116906}]
["ANAMET-M",7109294,"PG 29","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",1,20.996097669786842,{"$f":"F612*(1-Elteq!$F$5)","v":20.996097669786842}]
["ANAMET-M",7140124,"NPT 1/2\"","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",1,4.1620582991435864,{"$f":"F613*(1-Elteq!$F$5)","v":4.1620582991435864}]
["ANAMET-M",7140164,"NPT 1/2\"","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",1,4.673025277833089,{"$f":"F614*(1-Elteq!$F$5)","v":4.673025277833089}]
["ANAMET-M",7140204,"NPT 3/4\"","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",1,6.4660548575980705,{"$f":"F615*(1-Elteq!$F$5)","v":6.4660548575980705}]
["ANAMET-M",7140264,"NPT 1\"","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",1,11.324886309500069,{"$f":"F616*(1-Elteq!$F$5)","v":11.324886309500069}]
["ANAMET-M",7149124,"NPT 1/2\"","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",1,6.5682482533359723,{"$f":"F617*(1-Elteq!$F$5)","v":6.5682482533359723}]
["ANAMET-M",7149164,"NPT 1/2\"","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",1,7.8131496195976684,{"$f":"F618*(1-Elteq!$F$5)","v":7.8131496195976684}]
["ANAMET-M",7149204,"NPT 3/4\"","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",1,11.166951061541496,{"$f":"F619*(1-Elteq!$F$5)","v":11.166951061541496}]
["ANAMET-M",7149264,"NPT 1\"","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",1,20.698807791276582,{"$f":"F620*(1-Elteq!$F$5)","v":20.698807791276582}]
["ANAMET-M",8127164,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",1,12.021659462258482,{"$f":"F621*(1-Elteq!$F$5)","v":12.021659462258482}]
["ANAMET-M",8127174,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",1,12.161014092810165,{"$f":"F622*(1-Elteq!$F$5)","v":12.161014092810165}]
["ANAMET-M",8127204,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",1,14.827332690699025,{"$f":"F623*(1-Elteq!$F$5)","v":14.827332690699025}]
["ANAMET-M",8127224,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",1,18.487714319856554,{"$f":"F624*(1-Elteq!$F$5)","v":18.487714319856554}]
["ANAMET-M",8127254,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",1,23.170029906393086,{"$f":"F625*(1-Elteq!$F$5)","v":23.170029906393086}]
["ANAMET-M",8127284,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",1,25.631961712806145,{"$f":"F626*(1-Elteq!$F$5)","v":25.631961712806145}]
["ANAMET-M",8127324,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",1,59.086363353913406,{"$f":"F627*(1-Elteq!$F$5)","v":59.086363353913406}]
["ANAMET-M",8139154,"M16 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 65",1,15.672750782712566,{"$f":"F628*(1-Elteq!$F$5)","v":15.672750782712566}]
["ANAMET-M",8139164,"M16 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 65",1,13.823979350726912,{"$f":"F629*(1-Elteq!$F$5)","v":13.823979350726912}]
["ANAMET-M",8139204,"M20 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 65",1,17.902424871539484,{"$f":"F630*(1-Elteq!$F$5)","v":17.902424871539484}]
["ANAMET-M",8139254,"M25 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 65",1,28.753505437163835,{"$f":"F631*(1-Elteq!$F$5)","v":28.753505437163835}]
["ANAMET-M",8139324,"M32 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 65",1,46.284317960565502,{"$f":"F632*(1-Elteq!$F$5)","v":46.284317960565502}]
["ANAMET-M",2641100,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",1,1.4585784664409442,{"$f":"F633*(1-Elteq!$F$5)","v":1.4585784664409442}]
["ANAMET-M",2641120,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",1,1.5236106273650625,{"$f":"F634*(1-Elteq!$F$5)","v":1.5236106273650625}]
["ANAMET-M",2641160,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",1,1.9045132842063281,{"$f":"F635*(1-Elteq!$F$5)","v":1.9045132842063281}]
["ANAMET-M",2641180,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",1,1.9045132842063281,{"$f":"F636*(1-Elteq!$F$5)","v":1.9045132842063281}]
["ANAMET-M",2641200,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",1,2.3597384106751584,{"$f":"F637*(1-Elteq!$F$5)","v":2.3597384106751584}]
["ANAMET-M",2641250,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",1,3.2887692810197087,{"$f":"F638*(1-Elteq!$F$5)","v":3.2887692810197087}]
["ANAMET-M",2641320,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",1,4.8959926867157808,{"$f":"F639*(1-Elteq!$F$5)","v":4.8959926867157808}]
["ANAMET-M",7120165,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",1,4.0227036685919026,{"$f":"F640*(1-Elteq!$F$5)","v":4.0227036685919026}]
["ANAMET-M",7120175,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",1,4.3943160167297233,{"$f":"F641*(1-Elteq!$F$5)","v":4.3943160167297233}]
["ANAMET-M",7120205,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",1,4.635864043019307,{"$f":"F642*(1-Elteq!$F$5)","v":4.635864043019307}]
["ANAMET-M",7120255,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",1,7.1999892451702658,{"$f":"F643*(1-Elteq!$F$5)","v":7.1999892451702658}]
["ANAMET-M",7120325,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",1,11.464240940051752,{"$f":"F644*(1-Elteq!$F$5)","v":11.464240940051752}]
["ANAMET-M",7120405,"M40 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",1,21.84151576180038,{"$f":"F645*(1-Elteq!$F$5)","v":21.84151576180038}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},7129165,"M16 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",1,7.2371504799840478,{"$f":"F646*(1-Elteq!$F$5)","v":7.2371504799840478}]
["ANAMET-M",7129175,"M20 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",1,8.5099227723560809,{"$f":"F647*(1-Elteq!$F$5)","v":8.5099227723560809}]
["ANAMET-M",7129205,"M20 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",1,8.6306967855008718,{"$f":"F648*(1-Elteq!$F$5)","v":8.6306967855008718}]
["ANAMET-M",7129255,"M25 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",1,13.647463485361445,{"$f":"F649*(1-Elteq!$F$5)","v":13.647463485361445}]
["ANAMET-M",7129325,"M32 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",1,24.842285473013277,{"$f":"F650*(1-Elteq!$F$5)","v":24.842285473013277}]
["ANAMET-M",7840104,"-","Multiflex fittings for FCE / FCD, Conduit connector, IP 65",1,7.3021826409081667,{"$f":"F651*(1-Elteq!$F$5)","v":7.3021826409081667}]
["ANAMET-M",7840124,"-","Multiflex fittings for FCE / FCD, Conduit connector, IP 65",1,6.1873455964947057,{"$f":"F652*(1-Elteq!$F$5)","v":6.1873455964947057}]
["ANAMET-M",7840164,"-","Multiflex fittings for FCE / FCD, Conduit connector, IP 65",1,7.5251500497908586,{"$f":"F653*(1-Elteq!$F$5)","v":7.5251500497908586}]
["ANAMET-M",7840204,"-","Multiflex fittings for FCE / FCD, Conduit connector, IP 65",1,11.315596000796624,{"$f":"F654*(1-Elteq!$F$5)","v":11.315596000796624}]
["ANAMET-M",7840264,"-","Multiflex fittings for FCE / FCD, Conduit connector, IP 65",1,20.299324517028428,{"$f":"F655*(1-Elteq!$F$5)","v":20.299324517028428}]
["ANAMET-M",8120125,"M12 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",1,5.2397341087432645,{"$f":"F656*(1-Elteq!$F$5)","v":5.2397341087432645}]
["ANAMET-M",8130165,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 68",1,9.4389536427006338,{"$f":"F657*(1-Elteq!$F$5)","v":9.4389536427006338}]
["ANAMET-M",8130205,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 68",1,10.721016243776111,{"$f":"F658*(1-Elteq!$F$5)","v":10.721016243776111}]
["ANAMET-M",8130255,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 68",1,14.121269229237166,{"$f":"F659*(1-Elteq!$F$5)","v":14.121269229237166}]
["ANAMET-M",8130325,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 68",1,23.504481019717126,{"$f":"F660*(1-Elteq!$F$5)","v":23.504481019717126}]
["ANAMET-M",8199124,"NPT 1/2\"","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 68",1,15.951460043815931,{"$f":"F661*(1-Elteq!$F$5)","v":15.951460043815931}]
["ANAMET-M",8199164,"NPT 1/2\"","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 68",1,20.773130260904146,{"$f":"F662*(1-Elteq!$F$5)","v":20.773130260904146}]
["ANAMET-M",8199204,"NPT 3/4\"","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 68",1,29.682536307508382,{"$f":"F663*(1-Elteq!$F$5)","v":29.682536307508382}]
["ANAMET-M",8199264,"NPT 1\"","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 68",1,47.306251917944508,{"$f":"F664*(1-Elteq!$F$5)","v":47.306251917944508}]
["ANAMET-M",7100115,"PG 11","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",1,4.0877358295160224,{"$f":"F665*(1-Elteq!$F$5)","v":4.0877358295160224}]
["ANAMET-M",7100135,"PG 13,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",1,4.1063164469229125,{"$f":"F666*(1-Elteq!$F$5)","v":4.1063164469229125}]
["ANAMET-M",7100165,"PG 16","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",1,4.8402508344951078,{"$f":"F667*(1-Elteq!$F$5)","v":4.8402508344951078}]
["ANAMET-M",7100215,"PG 21","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",1,7.3486341844253937,{"$f":"F668*(1-Elteq!$F$5)","v":7.3486341844253937}]
["ANAMET-M",7100295,"PG 29","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",1,11.96591761003781,{"$f":"F669*(1-Elteq!$F$5)","v":11.96591761003781}]
["ANAMET-M",7109115,"PG 11","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",1,7.5344403584943027,{"$f":"F670*(1-Elteq!$F$5)","v":7.5344403584943027}]
["ANAMET-M",7109135,"PG 13,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",1,7.7666980760804405,{"$f":"F671*(1-Elteq!$F$5)","v":7.7666980760804405}]
["ANAMET-M",7109165,"PG 16","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",1,9.2066959251144951,{"$f":"F672*(1-Elteq!$F$5)","v":9.2066959251144951}]
["ANAMET-M",7109215,"PG 21","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",1,13.489528237402872,{"$f":"F673*(1-Elteq!$F$5)","v":13.489528237402872}]
["ANAMET-M",7109295,"PG 29","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",1,25.195317203744207,{"$f":"F674*(1-Elteq!$F$5)","v":25.195317203744207}]
["ANAMET-M",8103115,"PG 11","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",1,6.911989675363456,{"$f":"F675*(1-Elteq!$F$5)","v":6.911989675363456}]
["ANAMET-M",8103135,"PG 13,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",1,6.9119896753634551,{"$f":"F676*(1-Elteq!$F$5)","v":6.9119896753634551}]
["ANAMET-M",8103165,"PG 16","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",1,7.3672148018322838,{"$f":"F677*(1-Elteq!$F$5)","v":7.3672148018322838}]
["ANAMET-M",8103215,"PG 21","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",1,10.869661183031239,{"$f":"F678*(1-Elteq!$F$5)","v":10.869661183031239}]
["ANAMET-M",8103295,"PG 29","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",1,15.514815534753993,{"$f":"F679*(1-Elteq!$F$5)","v":15.514815534753993}]
["ANAMET-M",8107115,"PG 11","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",1,14.585784664409442,{"$f":"F680*(1-Elteq!$F$5)","v":14.585784664409442}]
["ANAMET-M",8107155,"PG 13,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",1,16.685394431388129,{"$f":"F681*(1-Elteq!$F$5)","v":16.685394431388129}]
["ANAMET-M",8107165,"PG 16","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",1,20.345776060545653,{"$f":"F682*(1-Elteq!$F$5)","v":20.345776060545653}]
["ANAMET-M",8107215,"PG 21","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",1,30.75092180840462,{"$f":"F683*(1-Elteq!$F$5)","v":30.75092180840462}]
["ANAMET-M",8107295,"PG 29","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",1,44.138256650069586,{"$f":"F684*(1-Elteq!$F$5)","v":44.138256650069586}]
["ANAMET-M",8123165,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",1,6.5961191794463083,{"$f":"F685*(1-Elteq!$F$5)","v":6.5961191794463083}]
["ANAMET-M",8123205,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",1,7.0885055407289199,{"$f":"F686*(1-Elteq!$F$5)","v":7.0885055407289199}]
["ANAMET-M",8123255,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",1,10.461630824775913,{"$f":"F687*(1-Elteq!$F$5)","v":10.461630824775913}]
["ANAMET-M",8123325,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",1,14.966687321250706,{"$f":"F688*(1-Elteq!$F$5)","v":14.966687321250706}]
["ANAMET-M",8127165,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",1,14.437139725154312,{"$f":"F689*(1-Elteq!$F$5)","v":14.437139725154312}]
["ANAMET-M",8127175,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",1,14.595074973112887,{"$f":"F690*(1-Elteq!$F$5)","v":14.595074973112887}]
["ANAMET-M",8127205,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",1,16.676104122684681,{"$f":"F691*(1-Elteq!$F$5)","v":16.676104122684681}]
["ANAMET-M",8127225,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",1,20.345776060545653,{"$f":"F692*(1-Elteq!$F$5)","v":20.345776060545653}]
["ANAMET-M",8127255,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",1,27.805893949412393,{"$f":"F693*(1-Elteq!$F$5)","v":27.805893949412393}]
["ANAMET-M",8127285,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",1,30.760212117108065,{"$f":"F694*(1-Elteq!$F$5)","v":30.760212117108065}]
["ANAMET-M",8127325,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",1,70.903636024696084,{"$f":"F695*(1-Elteq!$F$5)","v":70.903636024696084}]
["ANAMET-M",8139165,"M16 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 68",1,16.703975048795016,{"$f":"F696*(1-Elteq!$F$5)","v":16.703975048795016}]
["ANAMET-M",8139205,"M20 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 68",1,20.8660333479386,{"$f":"F697*(1-Elteq!$F$5)","v":20.8660333479386}]
["ANAMET-M",8139255,"M25 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 68",1,34.318400350527689,{"$f":"F698*(1-Elteq!$F$5)","v":34.318400350527689}]
["ANAMET-M",8139325,"M32 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 68",1,51.013085090619256,{"$f":"F699*(1-Elteq!$F$5)","v":51.013085090619256}]
["ANAMET-M",7140125,"NPT 1/2\"","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",1,4.9981860824536808,{"$f":"F700*(1-Elteq!$F$5)","v":4.9981860824536808}]
["ANAMET-M",7140165,"NPT 1/2\"","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",1,5.6113464568810842,{"$f":"F701*(1-Elteq!$F$5)","v":5.6113464568810842}]
["ANAMET-M",7140205,"NPT 3/4\"","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",1,7.7574077673769963,{"$f":"F702*(1-Elteq!$F$5)","v":7.7574077673769963}]
["ANAMET-M",7140265,"NPT 1\"","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",1,13.591721633140773,{"$f":"F703*(1-Elteq!$F$5)","v":13.591721633140773}]
["ANAMET-M",7149125,"NPT 1/2\"","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",1,7.8781817805217882,{"$f":"F704*(1-Elteq!$F$5)","v":7.8781817805217882}]
["ANAMET-M",7149165,"NPT 1/2\"","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",1,9.3739214817765131,{"$f":"F705*(1-Elteq!$F$5)","v":9.3739214817765131}]
["ANAMET-M",7149205,"NPT 3/4\"","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",1,13.396625150368417,{"$f":"F706*(1-Elteq!$F$5)","v":13.396625150368417}]
["ANAMET-M",7149265,"NPT 1\"","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",1,24.842285473013277,{"$f":"F707*(1-Elteq!$F$5)","v":24.842285473013277}]
["ANAMET-M",7840125,"-","Multiflex fittings for FCE / FCD, Conduit connector, IP 68",1,7.4229566540529577,{"$f":"F708*(1-Elteq!$F$5)","v":7.4229566540529577}]
["ANAMET-M",7840165,"-","Multiflex fittings for FCE / FCD, Conduit connector, IP 68",1,9.0301800597490303,{"$f":"F709*(1-Elteq!$F$5)","v":9.0301800597490303}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},7840205,"-","Multiflex fittings for FCE / FCD, Conduit connector, IP 68",1,13.582431324437325,{"$f":"F710*(1-Elteq!$F$5)","v":13.582431324437325}]
["ANAMET-M",7840265,"-","Multiflex fittings for FCE / FCD, Conduit connector, IP 68",1,24.359189420434113,{"$f":"F711*(1-Elteq!$F$5)","v":24.359189420434113}]
["ANAMET-M",8143125,"NPT 1/2\"","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",1,8.3241165982871728,{"$f":"F712*(1-Elteq!$F$5)","v":8.3241165982871728}]
["ANAMET-M",8143165,"NPT 1/2\"","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",1,8.9744382075283582,{"$f":"F713*(1-Elteq!$F$5)","v":8.9744382075283582}]
["ANAMET-M",8143205,"NPT 3/4\"","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",1,12.15172378410672,{"$f":"F714*(1-Elteq!$F$5)","v":12.15172378410672}]
["ANAMET-M",8143265,"NPT 1\"","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",1,15.171074112726506,{"$f":"F715*(1-Elteq!$F$5)","v":15.171074112726506}]
["ANAMET-M",2980126,"NPT 1/2\"","Aluminium fittings for Sealtite EFL, Straight fixed with male thread, IP 68",1,19.045132842063285,{"$f":"F716*(1-Elteq!$F$5)","v":19.045132842063285}]
["ANAMET-M",2980166,"NPT 1/2\"","Aluminium fittings for Sealtite EFL, Straight fixed with male thread, IP 68",1,21.460613104959116,{"$f":"F717*(1-Elteq!$F$5)","v":21.460613104959116}]
["ANAMET-M",2980206,"NPT 3/4\"","Aluminium fittings for Sealtite EFL, Straight fixed with male thread, IP 68",1,22.668353236407029,{"$f":"F718*(1-Elteq!$F$5)","v":22.668353236407029}]
["ANAMET-M",2980266,"NPT 1\"","Aluminium fittings for Sealtite EFL, Straight fixed with male thread, IP 68",1,42.549613861780408,{"$f":"F719*(1-Elteq!$F$5)","v":42.549613861780408}]
["ANAMET-M",2980356,"NPT 1 1/4\"","Aluminium fittings for Sealtite EFL, Straight fixed with male thread, IP 68",1,76.737949890459859,{"$f":"F720*(1-Elteq!$F$5)","v":76.737949890459859}]
["ANAMET-M",2989126,"NPT 1/2\"","Aluminium fittings for Sealtite EFL, 90° elbow fixed with male thread, IP 68",1,20.624485321649018,{"$f":"F721*(1-Elteq!$F$5)","v":20.624485321649018}]
["ANAMET-M",2989166,"NPT 1/2\"","Aluminium fittings for Sealtite EFL, 90° elbow fixed with male thread, IP 68",1,22.203837801234755,{"$f":"F722*(1-Elteq!$F$5)","v":22.203837801234755}]
["ANAMET-M",2989206,"NPT 3/4\"","Aluminium fittings for Sealtite EFL, 90° elbow fixed with male thread, IP 68",1,53.790887392949465,{"$f":"F723*(1-Elteq!$F$5)","v":53.790887392949465}]
["ANAMET-M",2989266,"NPT 1\"","Aluminium fittings for Sealtite EFL, 90° elbow fixed with male thread, IP 68",1,62.616680661222709,{"$f":"F724*(1-Elteq!$F$5)","v":62.616680661222709}]
["ANAMET-M",2989356,"NPT 1 1/4\"","Aluminium fittings for Sealtite EFL, 90° elbow fixed with male thread, IP 68",1,120.56962635331575,{"$f":"F725*(1-Elteq!$F$5)","v":120.56962635331575}]
["ANAMET-M",7100111,"PG 11","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,3.4095432941644996,{"$f":"F726*(1-Elteq!$F$5)","v":3.4095432941644996}]
["ANAMET-M",7100131,"PG 13,5","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,3.4188336028679456,{"$f":"F727*(1-Elteq!$F$5)","v":3.4188336028679456}]
["ANAMET-M",7100161,"PG 16","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,4.0319939772953486,{"$f":"F728*(1-Elteq!$F$5)","v":4.0319939772953486}]
["ANAMET-M",7100211,"PG 21","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,6.1223134355705868,{"$f":"F729*(1-Elteq!$F$5)","v":6.1223134355705868}]
["ANAMET-M",7100291,"PG 29","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,9.9592109300935814,{"$f":"F730*(1-Elteq!$F$5)","v":9.9592109300935814}]
["ANAMET-M",7100361,"PG 36","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,15.551976769567775,{"$f":"F731*(1-Elteq!$F$5)","v":15.551976769567775}]
["ANAMET-M",7100421,"PG 42","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,21.525645265883234,{"$f":"F732*(1-Elteq!$F$5)","v":21.525645265883234}]
["ANAMET-M",7100481,"PG 48","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,30.778792734514955,{"$f":"F733*(1-Elteq!$F$5)","v":30.778792734514955}]
["ANAMET-M",7109111,"PG 11","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,6.2709583748257147,{"$f":"F734*(1-Elteq!$F$5)","v":6.2709583748257147}]
["ANAMET-M",7109131,"PG 13,5","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,6.4753451663015156,{"$f":"F735*(1-Elteq!$F$5)","v":6.4753451663015156}]
["ANAMET-M",7109161,"PG 16","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,7.6645046803425414,{"$f":"F736*(1-Elteq!$F$5)","v":7.6645046803425414}]
["ANAMET-M",7109211,"PG 21","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,11.231983222465614,{"$f":"F737*(1-Elteq!$F$5)","v":11.231983222465614}]
["ANAMET-M",7109291,"PG 29","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,20.986807361083393,{"$f":"F738*(1-Elteq!$F$5)","v":20.986807361083393}]
["ANAMET-M",7109361,"PG 36","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,33.222143923521124,{"$f":"F739*(1-Elteq!$F$5)","v":33.222143923521124}]
["ANAMET-M",7109421,"PG 42","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,44.769997641903885,{"$f":"F740*(1-Elteq!$F$5)","v":44.769997641903885}]
["ANAMET-M",7109481,"PG 48","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,69.751637745468841,{"$f":"F741*(1-Elteq!$F$5)","v":69.751637745468841}]
["ANAMET-M",7120140,"M20 x 1,5","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,4.7752186735709889,{"$f":"F742*(1-Elteq!$F$5)","v":4.7752186735709889}]
["ANAMET-M",7120150,"M16 x 1,5","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,4.4686384863572872,{"$f":"F743*(1-Elteq!$F$5)","v":4.4686384863572872}]
["ANAMET-M",7120161,"M16 x 1,5","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,3.3538014419438267,{"$f":"F744*(1-Elteq!$F$5)","v":3.3538014419438267}]
["ANAMET-M",7120171,"M20 x 1,5","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,3.6603816291575288,{"$f":"F745*(1-Elteq!$F$5)","v":3.6603816291575288}]
["ANAMET-M",7120201,"M20 x 1,5","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,3.8647684206333297,{"$f":"F746*(1-Elteq!$F$5)","v":3.8647684206333297}]
["ANAMET-M",7120251,"M25 x 1,5","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,6.0015394224257959,{"$f":"F747*(1-Elteq!$F$5)","v":6.0015394224257959}]
["ANAMET-M",7120321,"M32 x 1,5","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,9.5504373471419779,{"$f":"F748*(1-Elteq!$F$5)","v":9.5504373471419779}]
["ANAMET-M",7120401,"M40 x 1,5","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,15.403331830312645,{"$f":"F749*(1-Elteq!$F$5)","v":15.403331830312645}]
["ANAMET-M",7120501,"M50 x 1,5","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,21.627838661621134,{"$f":"F750*(1-Elteq!$F$5)","v":21.627838661621134}]
["ANAMET-M",7120631,"M63 x 1,5","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,30.992469834694202,{"$f":"F751*(1-Elteq!$F$5)","v":30.992469834694202}]
["ANAMET-M",7124140,"M20 x 1,5","Compact fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,8.6864386377215457,{"$f":"F752*(1-Elteq!$F$5)","v":8.6864386377215457}]
["ANAMET-M",7124150,"M16 x 1,5","Compact fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,7.5716015933080856,{"$f":"F753*(1-Elteq!$F$5)","v":7.5716015933080856}]
["ANAMET-M",7124161,"M16 x 1,5","Compact fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,6.0294103485361328,{"$f":"F754*(1-Elteq!$F$5)","v":6.0294103485361328}]
["ANAMET-M",7124171,"M20 x 1,5","Compact fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,7.0885055407289199,{"$f":"F755*(1-Elteq!$F$5)","v":7.0885055407289199}]
["ANAMET-M",7124201,"M20 x 1,5","Compact fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,7.1906989364668199,{"$f":"F756*(1-Elteq!$F$5)","v":7.1906989364668199}]
["ANAMET-M",7124251,"M25 x 1,5","Compact fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,11.371337853017296,{"$f":"F757*(1-Elteq!$F$5)","v":11.371337853017296}]
["ANAMET-M",7124321,"M32 x 1,5","Compact fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,20.698807791276582,{"$f":"F758*(1-Elteq!$F$5)","v":20.698807791276582}]
["ANAMET-M",7129140,"M20 x 1,5","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,8.20334258514238,{"$f":"F759*(1-Elteq!$F$5)","v":8.20334258514238}]
["ANAMET-M",7129150,"M16 x 1,5","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,7.1442473929495938,{"$f":"F760*(1-Elteq!$F$5)","v":7.1442473929495938}]
["ANAMET-M",7129161,"M16 x 1,5","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,6.0294103485361328,{"$f":"F761*(1-Elteq!$F$5)","v":6.0294103485361328}]
["ANAMET-M",7129171,"M20 x 1,5","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,7.0885055407289199,{"$f":"F762*(1-Elteq!$F$5)","v":7.0885055407289199}]
["ANAMET-M",7129201,"M20 x 1,5","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,7.1906989364668199,{"$f":"F763*(1-Elteq!$F$5)","v":7.1906989364668199}]
["ANAMET-M",7129251,"M25 x 1,5","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,11.371337853017296,{"$f":"F764*(1-Elteq!$F$5)","v":11.371337853017296}]
["ANAMET-M",7129321,"M32 x 1,5","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,20.698807791276582,{"$f":"F765*(1-Elteq!$F$5)","v":20.698807791276582}]
["ANAMET-M",7129401,"M40 x 1,5","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,33.222143923521124,{"$f":"F766*(1-Elteq!$F$5)","v":33.222143923521124}]
["ANAMET-M",7129501,"M50 x 1,5","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,44.769997641903885,{"$f":"F767*(1-Elteq!$F$5)","v":44.769997641903885}]
["ANAMET-M",7129631,"M63 x 1,5","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,67.215383469428218,{"$f":"F768*(1-Elteq!$F$5)","v":67.215383469428218}]
["ANAMET-M",7140121,"NPT 1/2\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,3.5303173073092915,{"$f":"F769*(1-Elteq!$F$5)","v":3.5303173073092915}]
["ANAMET-M",7140122,"NPT 1/2\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,3.7904459510057658,{"$f":"F770*(1-Elteq!$F$5)","v":3.7904459510057658}]
["ANAMET-M",7140161,"NPT 1/2\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,4.0505745947022396,{"$f":"F771*(1-Elteq!$F$5)","v":4.0505745947022396}]
["ANAMET-M",7140162,"NPT 1/2\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,4.3014129296952683,{"$f":"F772*(1-Elteq!$F$5)","v":4.3014129296952683}]
["ANAMET-M",7140201,"NPT 3/4\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,5.6763786178052031,{"$f":"F773*(1-Elteq!$F$5)","v":5.6763786178052031}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},7140202,"NPT 3/4\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,6.0851522007568049,{"$f":"F774*(1-Elteq!$F$5)","v":6.0851522007568049}]
["ANAMET-M",7140261,"NPT 1\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,9.9777915475004715,{"$f":"F775*(1-Elteq!$F$5)","v":9.9777915475004715}]
["ANAMET-M",7140262,"NPT 1\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,10.572371304520985,{"$f":"F776*(1-Elteq!$F$5)","v":10.572371304520985}]
["ANAMET-M",7140351,"NPT 1.1/4\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,16.230169304919293,{"$f":"F777*(1-Elteq!$F$5)","v":16.230169304919293}]
["ANAMET-M",7140352,"NPT 1.1/4\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,17.224232336187963,{"$f":"F778*(1-Elteq!$F$5)","v":17.224232336187963}]
["ANAMET-M",7140401,"NPT 1.1/2\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,23.24435237602065,{"$f":"F779*(1-Elteq!$F$5)","v":23.24435237602065}]
["ANAMET-M",7140402,"NPT 1.1/2\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,24.479963433578902,{"$f":"F780*(1-Elteq!$F$5)","v":24.479963433578902}]
["ANAMET-M",7140501,"NPT 2\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,37.068331726747559,{"$f":"F781*(1-Elteq!$F$5)","v":37.068331726747559}]
["ANAMET-M",7140502,"NPT 2\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",1,38.833490380402203,{"$f":"F782*(1-Elteq!$F$5)","v":38.833490380402203}]
["ANAMET-M",7144121,"NPT 1/2\"","Compact fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,6.5589579446325255,{"$f":"F783*(1-Elteq!$F$5)","v":6.5589579446325255}]
["ANAMET-M",7144161,"NPT 1/2\"","Compact fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,7.8131496195976684,{"$f":"F784*(1-Elteq!$F$5)","v":7.8131496195976684}]
["ANAMET-M",7144201,"NPT 3/4\"","Compact fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,11.166951061541496,{"$f":"F785*(1-Elteq!$F$5)","v":11.166951061541496}]
["ANAMET-M",7144261,"NPT 1\"","Compact fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,20.698807791276582,{"$f":"F786*(1-Elteq!$F$5)","v":20.698807791276582}]
["ANAMET-M",7149121,"NPT 1/2\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,6.5589579446325255,{"$f":"F787*(1-Elteq!$F$5)","v":6.5589579446325255}]
["ANAMET-M",7149122,"NPT 1/2\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,6.8190865883289993,{"$f":"F788*(1-Elteq!$F$5)","v":6.8190865883289993}]
["ANAMET-M",7149161,"NPT 1/2\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,7.8131496195976684,{"$f":"F789*(1-Elteq!$F$5)","v":7.8131496195976684}]
["ANAMET-M",7149162,"NPT 1/2\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,8.0732782632941422,{"$f":"F790*(1-Elteq!$F$5)","v":8.0732782632941422}]
["ANAMET-M",7149201,"NPT 3/4\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,11.166951061541496,{"$f":"F791*(1-Elteq!$F$5)","v":11.166951061541496}]
["ANAMET-M",7149202,"NPT 3/4\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,11.5757246444931,{"$f":"F792*(1-Elteq!$F$5)","v":11.5757246444931}]
["ANAMET-M",7149261,"NPT 1\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,20.698807791276582,{"$f":"F793*(1-Elteq!$F$5)","v":20.698807791276582}]
["ANAMET-M",7149262,"NPT 1\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,21.293387548297098,{"$f":"F794*(1-Elteq!$F$5)","v":21.293387548297098}]
["ANAMET-M",7149351,"NPT 1.1/4\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,33.222143923521124,{"$f":"F795*(1-Elteq!$F$5)","v":33.222143923521124}]
["ANAMET-M",7149352,"NPT 1.1/4\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,34.21620695478979,{"$f":"F796*(1-Elteq!$F$5)","v":34.21620695478979}]
["ANAMET-M",7149401,"NPT 1.1/2\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,44.769997641903885,{"$f":"F797*(1-Elteq!$F$5)","v":44.769997641903885}]
["ANAMET-M",7149402,"NPT 1.1/2\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,46.005608699462137,{"$f":"F798*(1-Elteq!$F$5)","v":46.005608699462137}]
["ANAMET-M",7149501,"NPT 2\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,67.215383469428218,{"$f":"F799*(1-Elteq!$F$5)","v":67.215383469428218}]
["ANAMET-M",7149502,"NPT 2\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,68.971251814379414,{"$f":"F800*(1-Elteq!$F$5)","v":68.971251814379414}]
["ANAMET-M",8150112,"3/8\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,0.88257932682732287,{"$f":"F801*(1-Elteq!$F$5)","v":0.88257932682732287}]
["ANAMET-M",8150162,"1/2\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,0.93832117904799595,{"$f":"F802*(1-Elteq!$F$5)","v":0.93832117904799595}]
["ANAMET-M",8150212,"3/4\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,1.0033533399721144,{"$f":"F803*(1-Elteq!$F$5)","v":1.0033533399721144}]
["ANAMET-M",8150292,"1\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,1.0683855008962329,{"$f":"F804*(1-Elteq!$F$5)","v":1.0683855008962329}]
["ANAMET-M",8150362,"1.1/4\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,1.6165137143995176,{"$f":"F805*(1-Elteq!$F$5)","v":1.6165137143995176}]
["ANAMET-M",8150422,"1 1/2\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,2.1553516191993567,{"$f":"F806*(1-Elteq!$F$5)","v":2.1553516191993567}]
["ANAMET-M",8150482,"2\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,3.3816723680541636,{"$f":"F807*(1-Elteq!$F$5)","v":3.3816723680541636}]
["ANAMET-M",8130150,"M16 x 1,5","Swivel fittings for Sealtite, Straight swivel with male thread, IP 67",1,8.6121161680939817,{"$f":"F808*(1-Elteq!$F$5)","v":8.6121161680939817}]
["ANAMET-M",8130160,"M16 x 1,5","Swivel fittings for Sealtite, Straight swivel with male thread, IP 67",1,7.8688914718183423,{"$f":"F809*(1-Elteq!$F$5)","v":7.8688914718183423}]
["ANAMET-M",8130200,"M20 x 1,5","Swivel fittings for Sealtite, Straight swivel with male thread, IP 67",1,8.9372769727145744,{"$f":"F810*(1-Elteq!$F$5)","v":8.9372769727145744}]
["ANAMET-M",8130250,"M25 x 1,5","Swivel fittings for Sealtite, Straight swivel with male thread, IP 67",1,11.770821127265453,{"$f":"F811*(1-Elteq!$F$5)","v":11.770821127265453}]
["ANAMET-M",8130320,"M32 x 1,5","Swivel fittings for Sealtite, Straight swivel with male thread, IP 67",1,19.583970746863123,{"$f":"F812*(1-Elteq!$F$5)","v":19.583970746863123}]
["ANAMET-M",8130400,"M40 x 1,5","Swivel fittings for Sealtite, Straight swivel with male thread, IP 67",1,22.612611384186355,{"$f":"F813*(1-Elteq!$F$5)","v":22.612611384186355}]
["ANAMET-M",8130500,"M50 x 1,5","Swivel fittings for Sealtite, Straight swivel with male thread, IP 67",1,39.855424337781209,{"$f":"F814*(1-Elteq!$F$5)","v":39.855424337781209}]
["ANAMET-M",8130630,"M63 x 1,5","Swivel fittings for Sealtite, Straight swivel with male thread, IP 67",1,59.39294354112711,{"$f":"F815*(1-Elteq!$F$5)","v":59.39294354112711}]
["ANAMET-M",8134160,"M16 x 1,5","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",1,15.951460043815931,{"$f":"F816*(1-Elteq!$F$5)","v":15.951460043815931}]
["ANAMET-M",8134200,"M20 x 1,5","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",1,20.782420569607595,{"$f":"F817*(1-Elteq!$F$5)","v":20.782420569607595}]
["ANAMET-M",8134250,"M25 x 1,5","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",1,29.682536307508382,{"$f":"F818*(1-Elteq!$F$5)","v":29.682536307508382}]
["ANAMET-M",8134320,"M32 x 1,5","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",1,47.306251917944508,{"$f":"F819*(1-Elteq!$F$5)","v":47.306251917944508}]
["ANAMET-M",8139150,"M16 x 1,5","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",1,15.672750782712566,{"$f":"F820*(1-Elteq!$F$5)","v":15.672750782712566}]
["ANAMET-M",8139160,"M16 x 1,5","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",1,13.823979350726912,{"$f":"F821*(1-Elteq!$F$5)","v":13.823979350726912}]
["ANAMET-M",8139200,"M20 x 1,5","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",1,17.902424871539484,{"$f":"F822*(1-Elteq!$F$5)","v":17.902424871539484}]
["ANAMET-M",8139250,"M25 x 1,5","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",1,28.753505437163835,{"$f":"F823*(1-Elteq!$F$5)","v":28.753505437163835}]
["ANAMET-M",8139320,"M32 x 1,5","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",1,46.284317960565502,{"$f":"F824*(1-Elteq!$F$5)","v":46.284317960565502}]
["ANAMET-M",8194120,"NPT 1/2\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",1,15.951460043815931,{"$f":"F825*(1-Elteq!$F$5)","v":15.951460043815931}]
["ANAMET-M",8194160,"NPT 1/2\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",1,20.773130260904146,{"$f":"F826*(1-Elteq!$F$5)","v":20.773130260904146}]
["ANAMET-M",8194200,"NPT 3/4\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",1,29.682536307508382,{"$f":"F827*(1-Elteq!$F$5)","v":29.682536307508382}]
["ANAMET-M",8194260,"NPT 1\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",1,47.306251917944508,{"$f":"F828*(1-Elteq!$F$5)","v":47.306251917944508}]
["ANAMET-M",8199120,"NPT 1/2\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",1,15.951460043815931,{"$f":"F829*(1-Elteq!$F$5)","v":15.951460043815931}]
["ANAMET-M",8199160,"NPT 1/2\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",1,20.773130260904146,{"$f":"F830*(1-Elteq!$F$5)","v":20.773130260904146}]
["ANAMET-M",8199200,"NPT 3/4\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",1,29.682536307508382,{"$f":"F831*(1-Elteq!$F$5)","v":29.682536307508382}]
["ANAMET-M",8199260,"NPT 1\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",1,47.306251917944508,{"$f":"F832*(1-Elteq!$F$5)","v":47.306251917944508}]
["ANAMET-M",8120112,"M12 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,5.4069596654052834,{"$f":"F833*(1-Elteq!$F$5)","v":5.4069596654052834}]
["ANAMET-M",8120121,"M12 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,5.825023557060331,{"$f":"F834*(1-Elteq!$F$5)","v":5.825023557060331}]
["ANAMET-M",8120122,"M12 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,5.2397341087432645,{"$f":"F835*(1-Elteq!$F$5)","v":5.2397341087432645}]
["ANAMET-M",8120132,"M16 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,5.2397341087432645,{"$f":"F836*(1-Elteq!$F$5)","v":5.2397341087432645}]
["ANAMET-M",8120141,"M20 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,6.8376672057358912,{"$f":"F837*(1-Elteq!$F$5)","v":6.8376672057358912}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8120142,"M20 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,5.4069596654052834,{"$f":"F838*(1-Elteq!$F$5)","v":5.4069596654052834}]
["ANAMET-M",8120151,"M16 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,5.2954759609639375,{"$f":"F839*(1-Elteq!$F$5)","v":5.2954759609639375}]
["ANAMET-M",8120152,"M16 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,4.9796054650467907,{"$f":"F840*(1-Elteq!$F$5)","v":4.9796054650467907}]
["ANAMET-M",8120161,"M16 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,4.5801221907986331,{"$f":"F841*(1-Elteq!$F$5)","v":4.5801221907986331}]
["ANAMET-M",8120171,"M20 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,4.9238636128261177,{"$f":"F842*(1-Elteq!$F$5)","v":4.9238636128261177}]
["ANAMET-M",8120201,"M20 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,4.9238636128261177,{"$f":"F843*(1-Elteq!$F$5)","v":4.9238636128261177}]
["ANAMET-M",8120251,"M25 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,7.2650214060943847,{"$f":"F844*(1-Elteq!$F$5)","v":7.2650214060943847}]
["ANAMET-M",8120321,"M32 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,11.61288587930688,{"$f":"F845*(1-Elteq!$F$5)","v":11.61288587930688}]
["ANAMET-M",8120401,"M40 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,21.414161561441887,{"$f":"F846*(1-Elteq!$F$5)","v":21.414161561441887}]
["ANAMET-M",8120501,"M50 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,28.734924819756944,{"$f":"F847*(1-Elteq!$F$5)","v":28.734924819756944}]
["ANAMET-M",8120631,"M63 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,44.063934180442025,{"$f":"F848*(1-Elteq!$F$5)","v":44.063934180442025}]
["ANAMET-M",8123151,"M16 x 1,5","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,6.921279984066901,{"$f":"F849*(1-Elteq!$F$5)","v":6.921279984066901}]
["ANAMET-M",8123161,"M16 x 1,5","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,5.4998627524397383,{"$f":"F850*(1-Elteq!$F$5)","v":5.4998627524397383}]
["ANAMET-M",8123201,"M20 x 1,5","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,5.9086363353913409,{"$f":"F851*(1-Elteq!$F$5)","v":5.9086363353913409}]
["ANAMET-M",8123251,"M25 x 1,5","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,8.7143095638318844,{"$f":"F852*(1-Elteq!$F$5)","v":8.7143095638318844}]
["ANAMET-M",8123321,"M32 x 1,5","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,12.467594280023865,{"$f":"F853*(1-Elteq!$F$5)","v":12.467594280023865}]
["ANAMET-M",8123401,"M40 x 1,5","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,28.604860497908707,{"$f":"F854*(1-Elteq!$F$5)","v":28.604860497908707}]
["ANAMET-M",8123501,"M50 x 1,5","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,37.718653335988748,{"$f":"F855*(1-Elteq!$F$5)","v":37.718653335988748}]
["ANAMET-M",8123631,"M63 x 1,5","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,56.78236679545892,{"$f":"F856*(1-Elteq!$F$5)","v":56.78236679545892}]
["ANAMET-M",8124141,"M20 x 1,5","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,11.129789826727714,{"$f":"F857*(1-Elteq!$F$5)","v":11.129789826727714}]
["ANAMET-M",8124151,"M16 x 1,5","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,9.3088893208523942,{"$f":"F858*(1-Elteq!$F$5)","v":9.3088893208523942}]
["ANAMET-M",8124161,"M16 x 1,5","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,8.3519875243975079,{"$f":"F859*(1-Elteq!$F$5)","v":8.3519875243975079}]
["ANAMET-M",8124171,"M20 x 1,5","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,9.7083725951005508,{"$f":"F860*(1-Elteq!$F$5)","v":9.7083725951005508}]
["ANAMET-M",8124201,"M20 x 1,5","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,9.7083725951005508,{"$f":"F861*(1-Elteq!$F$5)","v":9.7083725951005508}]
["ANAMET-M",8124251,"M25 x 1,5","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,12.727722923720341,{"$f":"F862*(1-Elteq!$F$5)","v":12.727722923720341}]
["ANAMET-M",8124321,"M32 x 1,5","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,26.272993013343889,{"$f":"F863*(1-Elteq!$F$5)","v":26.272993013343889}]
["ANAMET-M",8124501,"M50 x 1,5","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,{"$error":"#VALUE!"},{"$f":"F864*(1-Elteq!$F$5)","v":{"$error":"#VALUE!"}}]
["ANAMET-M",8129141,"M20 x 1,5","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,11.129789826727714,{"$f":"F865*(1-Elteq!$F$5)","v":11.129789826727714}]
["ANAMET-M",8129151,"M16 x 1,5","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,9.7734047560246697,{"$f":"F866*(1-Elteq!$F$5)","v":9.7734047560246697}]
["ANAMET-M",8129161,"M16 x 1,5","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,8.3519875243975079,{"$f":"F867*(1-Elteq!$F$5)","v":8.3519875243975079}]
["ANAMET-M",8129171,"M20 x 1,5","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,9.7083725951005508,{"$f":"F868*(1-Elteq!$F$5)","v":9.7083725951005508}]
["ANAMET-M",8129201,"M20 x 1,5","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,9.7083725951005508,{"$f":"F869*(1-Elteq!$F$5)","v":9.7083725951005508}]
["ANAMET-M",8129251,"M25 x 1,5","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,12.727722923720341,{"$f":"F870*(1-Elteq!$F$5)","v":12.727722923720341}]
["ANAMET-M",8129321,"M32 x 1,5","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,26.272993013343889,{"$f":"F871*(1-Elteq!$F$5)","v":26.272993013343889}]
["ANAMET-M",7852340,"1/2”","Standard fittings for Sealtite, Multiple seals for cable hose fittings",1,1.0405145747858966,{"$f":"F872*(1-Elteq!$F$5)","v":1.0405145747858966}]
["ANAMET-M",7852350,"1/2”","Standard fittings for Sealtite, Multiple seals for cable hose fittings",1,1.0405145747858966,{"$f":"F873*(1-Elteq!$F$5)","v":1.0405145747858966}]
["ANAMET-M",7852430,"1/2”","Standard fittings for Sealtite, Multiple seals for cable hose fittings",1,1.0405145747858966,{"$f":"F874*(1-Elteq!$F$5)","v":1.0405145747858966}]
["ANAMET-M",7852440,"1/2”","Standard fittings for Sealtite, Multiple seals for cable hose fittings",1,1.0405145747858966,{"$f":"F875*(1-Elteq!$F$5)","v":1.0405145747858966}]
["ANAMET-M",7853270,"3/4”","Standard fittings for Sealtite, Multiple seals for cable hose fittings",1,1.1705788966341335,{"$f":"F876*(1-Elteq!$F$5)","v":1.1705788966341335}]
["ANAMET-M",7853366,"3/4”","Standard fittings for Sealtite, Multiple seals for cable hose fittings",1,1.1705788966341335,{"$f":"F877*(1-Elteq!$F$5)","v":1.1705788966341335}]
["ANAMET-M",7853380,"3/4”","Standard fittings for Sealtite, Multiple seals for cable hose fittings",1,1.1705788966341335,{"$f":"F878*(1-Elteq!$F$5)","v":1.1705788966341335}]
["ANAMET-M",7854375,"1”","Standard fittings for Sealtite, Multiple seals for cable hose fittings",1,1.8394811232822097,{"$f":"F879*(1-Elteq!$F$5)","v":1.8394811232822097}]
["ANAMET-M",7854480,"1”","Standard fittings for Sealtite, Multiple seals for cable hose fittings",1,1.8394811232822097,{"$f":"F880*(1-Elteq!$F$5)","v":1.8394811232822097}]
["ANAMET-M",7854650,"1”","Standard fittings for Sealtite, Multiple seals for cable hose fittings",1,1.8394811232822097,{"$f":"F881*(1-Elteq!$F$5)","v":1.8394811232822097}]
["ANAMET-M",7854660,"1”","Standard fittings for Sealtite, Multiple seals for cable hose fittings",1,1.8394811232822097,{"$f":"F882*(1-Elteq!$F$5)","v":1.8394811232822097}]
["ANAMET-M",8126152,"M16 x 1,5","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",1,19.305261485759761,{"$f":"F883*(1-Elteq!$F$5)","v":19.305261485759761}]
["ANAMET-M",8126161,"M16 x 1,5","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",1,19.305261485759761,{"$f":"F884*(1-Elteq!$F$5)","v":19.305261485759761}]
["ANAMET-M",8126171,"M16 x 1,5","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",1,19.305261485759761,{"$f":"F885*(1-Elteq!$F$5)","v":19.305261485759761}]
["ANAMET-M",8126201,"M20 x 1,5","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",1,22.408224592710557,{"$f":"F886*(1-Elteq!$F$5)","v":22.408224592710557}]
["ANAMET-M",8126221,"M25 x 1,5","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",1,28.511957410874253,{"$f":"F887*(1-Elteq!$F$5)","v":28.511957410874253}]
["ANAMET-M",8126281,"M32 x 1,5","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",1,40.39426224258105,{"$f":"F888*(1-Elteq!$F$5)","v":40.39426224258105}]
["ANAMET-M",8126351,"M40 x 1,5","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",1,62.737454674367491,{"$f":"F889*(1-Elteq!$F$5)","v":62.737454674367491}]
["ANAMET-M",8127152,"M16 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,12.021659462258482,{"$f":"F890*(1-Elteq!$F$5)","v":12.021659462258482}]
["ANAMET-M",8127161,"M16 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,12.021659462258482,{"$f":"F891*(1-Elteq!$F$5)","v":12.021659462258482}]
["ANAMET-M",8127162,"M16 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,14.38139787293364,{"$f":"F892*(1-Elteq!$F$5)","v":14.38139787293364}]
["ANAMET-M",8127171,"M20 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,12.021659462258482,{"$f":"F893*(1-Elteq!$F$5)","v":12.021659462258482}]
["ANAMET-M",8127201,"M20 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,13.898301820354476,{"$f":"F894*(1-Elteq!$F$5)","v":13.898301820354476}]
["ANAMET-M",8127202,"M20 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,16.471717331208879,{"$f":"F895*(1-Elteq!$F$5)","v":16.471717331208879}]
["ANAMET-M",8127221,"M25 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,17.558683449512003,{"$f":"F896*(1-Elteq!$F$5)","v":17.558683449512003}]
["ANAMET-M",8127252,"M25 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,23.160739597689641,{"$f":"F897*(1-Elteq!$F$5)","v":23.160739597689641}]
["ANAMET-M",8127281,"M32 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,27.740861788488274,{"$f":"F898*(1-Elteq!$F$5)","v":27.740861788488274}]
["ANAMET-M",8127322,"M32 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,59.086363353913399,{"$f":"F899*(1-Elteq!$F$5)","v":59.086363353913399}]
["ANAMET-M",8127351,"M40 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,41.63916360884275,{"$f":"F900*(1-Elteq!$F$5)","v":41.63916360884275}]
["ANAMET-M",8127402,"M40 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,77.917819095797455,{"$f":"F901*(1-Elteq!$F$5)","v":77.917819095797455}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8127502,"M50 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,112.04112296355278,{"$f":"F902*(1-Elteq!$F$5)","v":112.04112296355278}]
["ANAMET-M",8127632,"M63 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,168.67484481975657,{"$f":"F903*(1-Elteq!$F$5)","v":168.67484481975657}]
["ANAMET-M",8100071,"PG 7","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,5.834313865763777,{"$f":"F904*(1-Elteq!$F$5)","v":5.834313865763777}]
["ANAMET-M",8100072,"PG 7","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,5.2397341087432645,{"$f":"F905*(1-Elteq!$F$5)","v":5.2397341087432645}]
["ANAMET-M",8100091,"PG 9","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,6.2895389922326057,{"$f":"F906*(1-Elteq!$F$5)","v":6.2895389922326057}]
["ANAMET-M",8100092,"PG 9","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,5.2397341087432645,{"$f":"F907*(1-Elteq!$F$5)","v":5.2397341087432645}]
["ANAMET-M",8100101,"PG 9","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,4.756638056164098,{"$f":"F908*(1-Elteq!$F$5)","v":4.756638056164098}]
["ANAMET-M",8100111,"PG 11","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,4.8867023780123349,{"$f":"F909*(1-Elteq!$F$5)","v":4.8867023780123349}]
["ANAMET-M",8100121,"PG 11","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,6.2430874487153778,{"$f":"F910*(1-Elteq!$F$5)","v":6.2430874487153778}]
["ANAMET-M",8100131,"PG 13,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,4.8867023780123349,{"$f":"F911*(1-Elteq!$F$5)","v":4.8867023780123349}]
["ANAMET-M",8100141,"PG 13,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,6.3824420792670615,{"$f":"F912*(1-Elteq!$F$5)","v":6.3824420792670615}]
["ANAMET-M",8100161,"PG 16","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,5.7042495439155392,{"$f":"F913*(1-Elteq!$F$5)","v":5.7042495439155392}]
["ANAMET-M",8100211,"PG 21","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,7.5530209759011955,{"$f":"F914*(1-Elteq!$F$5)","v":7.5530209759011955}]
["ANAMET-M",8100291,"PG 29","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,13.006432184823705,{"$f":"F915*(1-Elteq!$F$5)","v":13.006432184823705}]
["ANAMET-M",8100361,"PG 36","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,21.414161561441887,{"$f":"F916*(1-Elteq!$F$5)","v":21.414161561441887}]
["ANAMET-M",8100421,"PG 42","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,28.734924819756944,{"$f":"F917*(1-Elteq!$F$5)","v":28.734924819756944}]
["ANAMET-M",8100481,"PG 48","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,44.063934180442025,{"$f":"F918*(1-Elteq!$F$5)","v":44.063934180442025}]
["ANAMET-M",8103111,"PG 11","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,5.759991396136213,{"$f":"F919*(1-Elteq!$F$5)","v":5.759991396136213}]
["ANAMET-M",8103121,"PG 11","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,7.1906989364668199,{"$f":"F920*(1-Elteq!$F$5)","v":7.1906989364668199}]
["ANAMET-M",8103131,"PG 13,5","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,5.759991396136213,{"$f":"F921*(1-Elteq!$F$5)","v":5.759991396136213}]
["ANAMET-M",8103141,"PG 13,5","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,7.1906989364668199,{"$f":"F922*(1-Elteq!$F$5)","v":7.1906989364668199}]
["ANAMET-M",8103161,"PG 16","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,6.1408940529774787,{"$f":"F923*(1-Elteq!$F$5)","v":6.1408940529774787}]
["ANAMET-M",8103211,"PG 21","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,9.0580509858593654,{"$f":"F924*(1-Elteq!$F$5)","v":9.0580509858593654}]
["ANAMET-M",8103291,"PG 29","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,12.913529097789251,{"$f":"F925*(1-Elteq!$F$5)","v":12.913529097789251}]
["ANAMET-M",8103361,"PG 36","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,28.604860497908707,{"$f":"F926*(1-Elteq!$F$5)","v":28.604860497908707}]
["ANAMET-M",8103421,"PG 42","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,41.137486938856696,{"$f":"F927*(1-Elteq!$F$5)","v":41.137486938856696}]
["ANAMET-M",8103481,"PG 48","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,56.78236679545892,{"$f":"F928*(1-Elteq!$F$5)","v":56.78236679545892}]
["ANAMET-M",8104111,"PG 11","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,8.3519875243975079,{"$f":"F929*(1-Elteq!$F$5)","v":8.3519875243975079}]
["ANAMET-M",8104121,"PG 11","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,10.126436486755599,{"$f":"F930*(1-Elteq!$F$5)","v":10.126436486755599}]
["ANAMET-M",8104131,"PG 13,5","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,8.6678580203146556,{"$f":"F931*(1-Elteq!$F$5)","v":8.6678580203146556}]
["ANAMET-M",8104141,"PG 13,5","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,10.126436486755599,{"$f":"F932*(1-Elteq!$F$5)","v":10.126436486755599}]
["ANAMET-M",8104161,"PG 16","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,10.033533399721145,{"$f":"F933*(1-Elteq!$F$5)","v":10.033533399721145}]
["ANAMET-M",8104211,"PG 21","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,13.192238358892617,{"$f":"F934*(1-Elteq!$F$5)","v":13.192238358892617}]
["ANAMET-M",8104291,"PG 29","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,27.313507588129781,{"$f":"F935*(1-Elteq!$F$5)","v":27.313507588129781}]
["ANAMET-M",8106091,"PG 9","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",1,20.735969026090366,{"$f":"F936*(1-Elteq!$F$5)","v":20.735969026090366}]
["ANAMET-M",8106111,"PG 11","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",1,19.305261485759761,{"$f":"F937*(1-Elteq!$F$5)","v":19.305261485759761}]
["ANAMET-M",8106121,"PG 9","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",1,19.305261485759761,{"$f":"F938*(1-Elteq!$F$5)","v":19.305261485759761}]
["ANAMET-M",8106151,"PG 13,5","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",1,19.305261485759761,{"$f":"F939*(1-Elteq!$F$5)","v":19.305261485759761}]
["ANAMET-M",8106161,"PG 16","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",1,22.408224592710557,{"$f":"F940*(1-Elteq!$F$5)","v":22.408224592710557}]
["ANAMET-M",8106211,"PG 21","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",1,40.39426224258105,{"$f":"F941*(1-Elteq!$F$5)","v":40.39426224258105}]
["ANAMET-M",8106291,"PG 29","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",1,62.737454674367491,{"$f":"F942*(1-Elteq!$F$5)","v":62.737454674367491}]
["ANAMET-M",8107091,"PG 9","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,13.675334411471782,{"$f":"F943*(1-Elteq!$F$5)","v":13.675334411471782}]
["ANAMET-M",8107111,"PG 11","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,12.021659462258482,{"$f":"F944*(1-Elteq!$F$5)","v":12.021659462258482}]
["ANAMET-M",8107121,"PG 9","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,12.021659462258482,{"$f":"F945*(1-Elteq!$F$5)","v":12.021659462258482}]
["ANAMET-M",8107151,"PG 13,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,13.898301820354476,{"$f":"F946*(1-Elteq!$F$5)","v":13.898301820354476}]
["ANAMET-M",8107161,"PG 16","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,17.558683449512003,{"$f":"F947*(1-Elteq!$F$5)","v":17.558683449512003}]
["ANAMET-M",8107211,"PG 21","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,27.740861788488274,{"$f":"F948*(1-Elteq!$F$5)","v":27.740861788488274}]
["ANAMET-M",8107291,"PG 29","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,41.63916360884275,{"$f":"F949*(1-Elteq!$F$5)","v":41.63916360884275}]
["ANAMET-M",8109111,"PG 11","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,8.3519875243975079,{"$f":"F950*(1-Elteq!$F$5)","v":8.3519875243975079}]
["ANAMET-M",8109121,"PG 11","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,10.126436486755599,{"$f":"F951*(1-Elteq!$F$5)","v":10.126436486755599}]
["ANAMET-M",8109131,"PG 13,5","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,8.6678580203146556,{"$f":"F952*(1-Elteq!$F$5)","v":8.6678580203146556}]
["ANAMET-M",8109141,"PG 13,5","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,10.126436486755599,{"$f":"F953*(1-Elteq!$F$5)","v":10.126436486755599}]
["ANAMET-M",8109161,"PG 16","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,10.033533399721145,{"$f":"F954*(1-Elteq!$F$5)","v":10.033533399721145}]
["ANAMET-M",8109211,"PG 21","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,13.192238358892617,{"$f":"F955*(1-Elteq!$F$5)","v":13.192238358892617}]
["ANAMET-M",8109291,"PG 29","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,27.313507588129781,{"$f":"F956*(1-Elteq!$F$5)","v":27.313507588129781}]
["ANAMET-M",8140111,"NPT 1/2\"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,6.5032160924118525,{"$f":"F957*(1-Elteq!$F$5)","v":6.5032160924118525}]
["ANAMET-M",8140121,"NPT 1/2\"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,5.2676050348536014,{"$f":"F958*(1-Elteq!$F$5)","v":5.2676050348536014}]
["ANAMET-M",8140161,"NPT 1/2\"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,5.5463142959569653,{"$f":"F959*(1-Elteq!$F$5)","v":5.5463142959569653}]
["ANAMET-M",8140201,"NPT 3/4\"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,7.1070861581358109,{"$f":"F960*(1-Elteq!$F$5)","v":7.1070861581358109}]
["ANAMET-M",8140261,"NPT 1 \"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,11.798692053375788,{"$f":"F961*(1-Elteq!$F$5)","v":11.798692053375788}]
["ANAMET-M",8140351,"NPT 1.1/4 \"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,22.19454749253131,{"$f":"F962*(1-Elteq!$F$5)","v":22.19454749253131}]
["ANAMET-M",8140401,"NPT 1.1/2\"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,31.670662370045729,{"$f":"F963*(1-Elteq!$F$5)","v":31.670662370045729}]
["ANAMET-M",8140501,"NPT 2\"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,49.78676434176446,{"$f":"F964*(1-Elteq!$F$5)","v":49.78676434176446}]
["ANAMET-M",8144111,"NPT 1/2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,10.107855869348709,{"$f":"F965*(1-Elteq!$F$5)","v":10.107855869348709}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8144121,"NPT 1/2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,8.6864386377215457,{"$f":"F966*(1-Elteq!$F$5)","v":8.6864386377215457}]
["ANAMET-M",8144161,"NPT 1/2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,9.281018394742059,{"$f":"F967*(1-Elteq!$F$5)","v":9.281018394742059}]
["ANAMET-M",8144201,"NPT 3/4\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,12.560497367058321,{"$f":"F968*(1-Elteq!$F$5)","v":12.560497367058321}]
["ANAMET-M",8144261,"NPT 1 \"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,23.1514492889862,{"$f":"F969*(1-Elteq!$F$5)","v":23.1514492889862}]
["ANAMET-M",8149111,"NPT 1/2\"","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,10.107855869348709,{"$f":"F970*(1-Elteq!$F$5)","v":10.107855869348709}]
["ANAMET-M",8149121,"NPT 1/2\"","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,8.6864386377215457,{"$f":"F971*(1-Elteq!$F$5)","v":8.6864386377215457}]
["ANAMET-M",8149161,"NPT 1/2\"","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,9.7548241386177796,{"$f":"F972*(1-Elteq!$F$5)","v":9.7548241386177796}]
["ANAMET-M",8149201,"NPT 3/4\"","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,13.006432184823705,{"$f":"F973*(1-Elteq!$F$5)","v":13.006432184823705}]
["ANAMET-M",8149261,"NPT 1 \"","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,23.1514492889862,{"$f":"F974*(1-Elteq!$F$5)","v":23.1514492889862}]
["ANAMET-M",8143111,"NPT 1/2\"","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,7.1906989364668199,{"$f":"F975*(1-Elteq!$F$5)","v":7.1906989364668199}]
["ANAMET-M",8143121,"NPT 1/2\"","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,5.759991396136213,{"$f":"F976*(1-Elteq!$F$5)","v":5.759991396136213}]
["ANAMET-M",8143161,"NPT 1/2\"","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,6.1873455964947057,{"$f":"F977*(1-Elteq!$F$5)","v":6.1873455964947057}]
["ANAMET-M",8143201,"NPT 3/4\"","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,9.1416637641903744,{"$f":"F978*(1-Elteq!$F$5)","v":9.1416637641903744}]
["ANAMET-M",8143261,"NPT 1 \"","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,13.062174037044379,{"$f":"F979*(1-Elteq!$F$5)","v":13.062174037044379}]
["ANAMET-M",8143351,"NPT 1.1/4 \"","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,28.837118215494844,{"$f":"F980*(1-Elteq!$F$5)","v":28.837118215494844}]
["ANAMET-M",8143401,"NPT 1.1/2\"","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,42.159420896235694,{"$f":"F981*(1-Elteq!$F$5)","v":42.159420896235694}]
["ANAMET-M",8143501,"NPT 2\"","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",1,64.103130053773981,{"$f":"F982*(1-Elteq!$F$5)","v":64.103130053773981}]
["ANAMET-M",8147091,"NPT 3/8\"","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,13.45236700258909,{"$f":"F983*(1-Elteq!$F$5)","v":13.45236700258909}]
["ANAMET-M",8147101,"NPT 3/8\"","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,12.021659462258482,{"$f":"F984*(1-Elteq!$F$5)","v":12.021659462258482}]
["ANAMET-M",8147121,"NPT 1/2\"","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,12.021659462258482,{"$f":"F985*(1-Elteq!$F$5)","v":12.021659462258482}]
["ANAMET-M",8147151,"NPT 1/2\"","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,17.558683449512003,{"$f":"F986*(1-Elteq!$F$5)","v":17.558683449512003}]
["ANAMET-M",8147211,"NPT 3/4\"","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",1,27.740861788488274,{"$f":"F987*(1-Elteq!$F$5)","v":27.740861788488274}]
["ANAMET-M",8150060,"1/4\"","Standard fittings for Sealtite, Ferrule, nickel plated brass",1,2.4340608803027224,{"$f":"F988*(1-Elteq!$F$5)","v":2.4340608803027224}]
["ANAMET-M",8150100,"5/16\"","Standard fittings for Sealtite, Ferrule, nickel plated brass",1,2.4340608803027224,{"$f":"F989*(1-Elteq!$F$5)","v":2.4340608803027224}]
["ANAMET-M",8150110,"3/8\"","Standard fittings for Sealtite, Ferrule, galvanised steel",1,1.1055467357100148,{"$f":"F990*(1-Elteq!$F$5)","v":1.1055467357100148}]
["ANAMET-M",8150113,"3/8\"","Standard fittings for Sealtite, Ferrule, nickel plated brass",1,2.7685119936267601,{"$f":"F991*(1-Elteq!$F$5)","v":2.7685119936267601}]
["ANAMET-M",8150160,"1/2\"","Standard fittings for Sealtite, Ferrule, galvanised steel",1,1.1705788966341335,{"$f":"F992*(1-Elteq!$F$5)","v":1.1705788966341335}]
["ANAMET-M",8150163,"1/2\"","Standard fittings for Sealtite, Ferrule, nickel plated brass",1,3.3352208245369357,{"$f":"F993*(1-Elteq!$F$5)","v":3.3352208245369357}]
["ANAMET-M",8150210,"3/4\"","Standard fittings for Sealtite, Ferrule, galvanised steel",1,1.2449013662616977,{"$f":"F994*(1-Elteq!$F$5)","v":1.2449013662616977}]
["ANAMET-M",8150213,"3/4\"","Standard fittings for Sealtite, Ferrule, nickel plated brass",1,3.9669618163712301,{"$f":"F995*(1-Elteq!$F$5)","v":3.9669618163712301}]
["ANAMET-M",8150290,"1\"","Standard fittings for Sealtite, Ferrule, galvanised steel",1,1.3378044532961524,{"$f":"F996*(1-Elteq!$F$5)","v":1.3378044532961524}]
["ANAMET-M",8150293,"1\"","Standard fittings for Sealtite, Ferrule, nickel plated brass",1,5.3140565783708276,{"$f":"F997*(1-Elteq!$F$5)","v":5.3140565783708276}]
["ANAMET-M",8150363,"1 1/4\"","Standard fittings for Sealtite, Ferrule, nickel plated brass",1,6.9770218362875731,{"$f":"F998*(1-Elteq!$F$5)","v":6.9770218362875731}]
["ANAMET-M",8150423,"1 1/2\"","Standard fittings for Sealtite, Ferrule, nickel plated brass",1,9.6247598167695418,{"$f":"F999*(1-Elteq!$F$5)","v":9.6247598167695418}]
["ANAMET-M",8150483,"2\"","Standard fittings for Sealtite, Ferrule, nickel plated brass",1,14.455720342561206,{"$f":"F1000*(1-Elteq!$F$5)","v":14.455720342561206}]
["ANAMET-M",8154160,"M 16","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.40877358295160221,{"$f":"F1001*(1-Elteq!$F$5)","v":0.40877358295160221}]
["ANAMET-M",8154200,"M 20","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.44593481776538418,{"$f":"F1002*(1-Elteq!$F$5)","v":0.44593481776538418}]
["ANAMET-M",8154250,"M 25","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.46451543517227523,{"$f":"F1003*(1-Elteq!$F$5)","v":0.46451543517227523}]
["ANAMET-M",8154320,"M 32","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.48309605257916621,{"$f":"F1004*(1-Elteq!$F$5)","v":0.48309605257916621}]
["ANAMET-M",8154400,"M 40","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.72464407886874938,{"$f":"F1005*(1-Elteq!$F$5)","v":0.72464407886874938}]
["ANAMET-M",8154500,"M 50","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,1.1148370444134605,{"$f":"F1006*(1-Elteq!$F$5)","v":1.1148370444134605}]
["ANAMET-M",8154630,"M 63","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,1.6165137143995176,{"$f":"F1007*(1-Elteq!$F$5)","v":1.6165137143995176}]
["ANAMET-M",8155070,"PG 7 / - / -","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.39948327424815672,{"$f":"F1008*(1-Elteq!$F$5)","v":0.39948327424815672}]
["ANAMET-M",8155090,"PG 9 / M16/ -","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.39948327424815672,{"$f":"F1009*(1-Elteq!$F$5)","v":0.39948327424815672}]
["ANAMET-M",8155110,"PG 11 / - / -","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.40877358295160221,{"$f":"F1010*(1-Elteq!$F$5)","v":0.40877358295160221}]
["ANAMET-M",8155130,"PG 13,5 / - / -","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.43664450906193863,{"$f":"F1011*(1-Elteq!$F$5)","v":0.43664450906193863}]
["ANAMET-M",8155160,"PG 16 / - / 1/2\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.44593481776538418,{"$f":"F1012*(1-Elteq!$F$5)","v":0.44593481776538418}]
["ANAMET-M",8155210,"PG 21 /  - / 3/4\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.46451543517227523,{"$f":"F1013*(1-Elteq!$F$5)","v":0.46451543517227523}]
["ANAMET-M",8155290,"PG 29 / - / 1\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.48309605257916621,{"$f":"F1014*(1-Elteq!$F$5)","v":0.48309605257916621}]
["ANAMET-M",8155360,"PG 36 / - / 1 1/4\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.72464407886874938,{"$f":"F1015*(1-Elteq!$F$5)","v":0.72464407886874938}]
["ANAMET-M",8155420,"PG 42 / - / 1 1/2\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,1.1148370444134605,{"$f":"F1016*(1-Elteq!$F$5)","v":1.1148370444134605}]
["ANAMET-M",8155480,"PG 48 / - / 2\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,1.6165137143995176,{"$f":"F1017*(1-Elteq!$F$5)","v":1.6165137143995176}]
["ANAMET-M",7120149,"M20 x 1,5","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,24.312737876916884,{"$f":"F1018*(1-Elteq!$F$5)","v":24.312737876916884}]
["ANAMET-M",7120159,"M16 x 1,5","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,18.078940736904951,{"$f":"F1019*(1-Elteq!$F$5)","v":18.078940736904951}]
["ANAMET-M",7120169,"M16 x 1,5","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,18.078940736904951,{"$f":"F1020*(1-Elteq!$F$5)","v":18.078940736904951}]
["ANAMET-M",7120179,"M20 x 1,5","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,24.312737876916884,{"$f":"F1021*(1-Elteq!$F$5)","v":24.312737876916884}]
["ANAMET-M",7120209,"M20 x 1,5","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,24.312737876916884,{"$f":"F1022*(1-Elteq!$F$5)","v":24.312737876916884}]
["ANAMET-M",7120259,"M25 x 1,5","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,28.939311611232743,{"$f":"F1023*(1-Elteq!$F$5)","v":28.939311611232743}]
["ANAMET-M",7120329,"M32 x 1,5","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,36.064978386775444,{"$f":"F1024*(1-Elteq!$F$5)","v":36.064978386775444}]
["ANAMET-M",7120409,"M40 x 1,5","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,53.270630105556521,{"$f":"F1025*(1-Elteq!$F$5)","v":53.270630105556521}]
["ANAMET-M",7120509,"M50 x 1,5","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,79.785171145189977,{"$f":"F1026*(1-Elteq!$F$5)","v":79.785171145189977}]
["ANAMET-M",7120639,"M63 x 1,5","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,113.81557192591087,{"$f":"F1027*(1-Elteq!$F$5)","v":113.81557192591087}]
["ANAMET-M",7129169,"M16 x 1,5","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,36.232203943437462,{"$f":"F1028*(1-Elteq!$F$5)","v":36.232203943437462}]
["ANAMET-M",7129179,"M20 x 1,5","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,37.347040987850924,{"$f":"F1029*(1-Elteq!$F$5)","v":37.347040987850924}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},7129209,"M20 x 1,5","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,41.137486938856696,{"$f":"F1030*(1-Elteq!$F$5)","v":41.137486938856696}]
["ANAMET-M",7129259,"M25 x 1,5","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,52.954759609639375,{"$f":"F1031*(1-Elteq!$F$5)","v":52.954759609639375}]
["ANAMET-M",7129329,"M32 x 1,5","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,79.487881266679736,{"$f":"F1032*(1-Elteq!$F$5)","v":79.487881266679736}]
["ANAMET-M",7129409,"M40 x 1,5","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,102.00758956383163,{"$f":"F1033*(1-Elteq!$F$5)","v":102.00758956383163}]
["ANAMET-M",7129509,"M50 x 1,5","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,146.04365281816331,{"$f":"F1034*(1-Elteq!$F$5)","v":146.04365281816331}]
["ANAMET-M",7129639,"M63 x 1,5","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,209.58936434973057,{"$f":"F1035*(1-Elteq!$F$5)","v":209.58936434973057}]
["ANAMET-M",7140129,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,18.078940736904951,{"$f":"F1036*(1-Elteq!$F$5)","v":18.078940736904951}]
["ANAMET-M",7140169,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,24.312737876916884,{"$f":"F1037*(1-Elteq!$F$5)","v":24.312737876916884}]
["ANAMET-M",7140209,"NPT 3/4\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,28.939311611232743,{"$f":"F1038*(1-Elteq!$F$5)","v":28.939311611232743}]
["ANAMET-M",7140269,"NPT 1\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,36.064978386775444,{"$f":"F1039*(1-Elteq!$F$5)","v":36.064978386775444}]
["ANAMET-M",7140359,"NPT 1.1/4\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,53.270630105556521,{"$f":"F1040*(1-Elteq!$F$5)","v":53.270630105556521}]
["ANAMET-M",7140409,"NPT 1.1/2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,79.785171145189977,{"$f":"F1041*(1-Elteq!$F$5)","v":79.785171145189977}]
["ANAMET-M",7140509,"NPT 2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,113.81557192591087,{"$f":"F1042*(1-Elteq!$F$5)","v":113.81557192591087}]
["ANAMET-M",7149129,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,36.232203943437462,{"$f":"F1043*(1-Elteq!$F$5)","v":36.232203943437462}]
["ANAMET-M",7149169,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,41.137486938856696,{"$f":"F1044*(1-Elteq!$F$5)","v":41.137486938856696}]
["ANAMET-M",7149209,"NPT 3/4\"","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,52.954759609639375,{"$f":"F1045*(1-Elteq!$F$5)","v":52.954759609639375}]
["ANAMET-M",7149269,"NPT 1\"","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,79.487881266679736,{"$f":"F1046*(1-Elteq!$F$5)","v":79.487881266679736}]
["ANAMET-M",7149359,"NPT 1.1/4\"","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,102.00758956383163,{"$f":"F1047*(1-Elteq!$F$5)","v":102.00758956383163}]
["ANAMET-M",7149409,"NPT 1.1/2\"","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,146.04365281816331,{"$f":"F1048*(1-Elteq!$F$5)","v":146.04365281816331}]
["ANAMET-M",7149509,"NPT 2\"","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,209.58936434973057,{"$f":"F1049*(1-Elteq!$F$5)","v":209.58936434973057}]
["ANAMET-M","7140129-2","NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,21.191194152559191,{"$f":"F1050*(1-Elteq!$F$5)","v":21.191194152559191}]
["ANAMET-M","7140169-2","NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,27.480733144791802,{"$f":"F1051*(1-Elteq!$F$5)","v":27.480733144791802}]
["ANAMET-M","7140209-2","NPT 3/4\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,32.05156502688699,{"$f":"F1052*(1-Elteq!$F$5)","v":32.05156502688699}]
["ANAMET-M","7140269-2","NPT 1\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,41.044583851822239,{"$f":"F1053*(1-Elteq!$F$5)","v":41.044583851822239}]
["ANAMET-M","7140359-2","NPT 1.1/4\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,59.597330332602915,{"$f":"F1054*(1-Elteq!$F$5)","v":59.597330332602915}]
["ANAMET-M","7140409-2","NPT 1.1/2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,88.973286452897597,{"$f":"F1055*(1-Elteq!$F$5)","v":88.973286452897597}]
["ANAMET-M","7140509-2","NPT 2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,128.75438832105124,{"$f":"F1056*(1-Elteq!$F$5)","v":128.75438832105124}]
["ANAMET-M","7149129-2","NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,39.344457359091713,{"$f":"F1057*(1-Elteq!$F$5)","v":39.344457359091713}]
["ANAMET-M","7149169-2","NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,44.249740354510941,{"$f":"F1058*(1-Elteq!$F$5)","v":44.249740354510941}]
["ANAMET-M","7149-209-2","NPT 3/4\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,56.122754877514289,{"$f":"F1059*(1-Elteq!$F$5)","v":56.122754877514289}]
["ANAMET-M","7149-269-2","NPT 1\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,84.467486731726524,{"$f":"F1060*(1-Elteq!$F$5)","v":84.467486731726524}]
["ANAMET-M","7149359-2","NPT 1.1/4\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,108.67803121290551,{"$f":"F1061*(1-Elteq!$F$5)","v":108.67803121290551}]
["ANAMET-M","7149409-2","NPT 1.1/2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,155.23176812587093,{"$f":"F1062*(1-Elteq!$F$5)","v":155.23176812587093}]
["ANAMET-M","7149509-2","NPT 2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,224.52818074487095,{"$f":"F1063*(1-Elteq!$F$5)","v":224.52818074487095}]
["ANAMET-M",8120149,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,31.401243417645798,{"$f":"F1064*(1-Elteq!$F$5)","v":31.401243417645798}]
["ANAMET-M",8120159,"M16 x 1,5","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,22.696224162517368,{"$f":"F1065*(1-Elteq!$F$5)","v":22.696224162517368}]
["ANAMET-M",8120169,"M16 x 1,5","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,21.265516622186759,{"$f":"F1066*(1-Elteq!$F$5)","v":21.265516622186759}]
["ANAMET-M",8120179,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,29.970535877315193,{"$f":"F1067*(1-Elteq!$F$5)","v":29.970535877315193}]
["ANAMET-M",8120209,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,29.970535877315193,{"$f":"F1068*(1-Elteq!$F$5)","v":29.970535877315193}]
["ANAMET-M",8120259,"M25 x 1,5","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,34.467045289782824,{"$f":"F1069*(1-Elteq!$F$5)","v":34.467045289782824}]
["ANAMET-M",8120329,"M 32 x 1,5","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,42.521742935670076,{"$f":"F1070*(1-Elteq!$F$5)","v":42.521742935670076}]
["ANAMET-M",8120409,"M40 x 1,5","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,88.583093487352869,{"$f":"F1071*(1-Elteq!$F$5)","v":88.583093487352869}]
["ANAMET-M",8124149,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 45° elbow, IP 67",1,53.233468870742733,{"$f":"F1072*(1-Elteq!$F$5)","v":53.233468870742733}]
["ANAMET-M",8124159,"M16 x 1,5","Standard fittings for Sealtite, Stainless steel 304 45° elbow, IP 67",1,38.183168771161029,{"$f":"F1073*(1-Elteq!$F$5)","v":38.183168771161029}]
["ANAMET-M",8124169,"M16 x 1,5","Standard fittings for Sealtite, Stainless steel 304 45° elbow, IP 67",1,36.761751539533861,{"$f":"F1074*(1-Elteq!$F$5)","v":36.761751539533861}]
["ANAMET-M",8124179,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 45° elbow, IP 67",1,51.81205163911558,{"$f":"F1075*(1-Elteq!$F$5)","v":51.81205163911558}]
["ANAMET-M",8124209,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 45° elbow, IP 67",1,51.81205163911558,{"$f":"F1076*(1-Elteq!$F$5)","v":51.81205163911558}]
["ANAMET-M",8124259,"M25 x 1,5","Standard fittings for Sealtite, Stainless steel 304 45° elbow, IP 67",1,59.569459406492577,{"$f":"F1077*(1-Elteq!$F$5)","v":59.569459406492577}]
["ANAMET-M",8127159,"M16 x 1,5","Standard fittings for Sealtite, Stainless steel 304 cablehose, IP 67",1,45.671157586138094,{"$f":"F1078*(1-Elteq!$F$5)","v":45.671157586138094}]
["ANAMET-M",8127169,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 cablehose, IP 67",1,44.240450045807485,{"$f":"F1079*(1-Elteq!$F$5)","v":44.240450045807485}]
["ANAMET-M",8127179,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 cablehose, IP 67",1,47.380574387572075,{"$f":"F1080*(1-Elteq!$F$5)","v":47.380574387572075}]
["ANAMET-M",8127209,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 cablehose, IP 67",1,52.304438000398186,{"$f":"F1081*(1-Elteq!$F$5)","v":52.304438000398186}]
["ANAMET-M",8129149,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,53.233468870742733,{"$f":"F1082*(1-Elteq!$F$5)","v":53.233468870742733}]
["ANAMET-M",8129159,"M16 x 1,5","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,38.183168771161029,{"$f":"F1083*(1-Elteq!$F$5)","v":38.183168771161029}]
["ANAMET-M",8129169,"M16 x 1,5","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,36.761751539533861,{"$f":"F1084*(1-Elteq!$F$5)","v":36.761751539533861}]
["ANAMET-M",8129179,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,51.81205163911558,{"$f":"F1085*(1-Elteq!$F$5)","v":51.81205163911558}]
["ANAMET-M",8129209,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,51.81205163911558,{"$f":"F1086*(1-Elteq!$F$5)","v":51.81205163911558}]
["ANAMET-M",8129259,"M25 x 1,5","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,59.569459406492577,{"$f":"F1087*(1-Elteq!$F$5)","v":59.569459406492577}]
["ANAMET-M",8150115,"3/8\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",1,3.1679952678749173,{"$f":"F1088*(1-Elteq!$F$5)","v":3.1679952678749173}]
["ANAMET-M",8150165,"1/2\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",1,3.7904459510057658,{"$f":"F1089*(1-Elteq!$F$5)","v":3.7904459510057658}]
["ANAMET-M",8150215,"3/4\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",1,4.4407675602469512,{"$f":"F1090*(1-Elteq!$F$5)","v":4.4407675602469512}]
["ANAMET-M",8150295,"1\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",1,5.0632182433777997,{"$f":"F1091*(1-Elteq!$F$5)","v":5.0632182433777997}]
["ANAMET-M",8150365,"1 1/4\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",1,5.4069596654052834,{"$f":"F1092*(1-Elteq!$F$5)","v":5.4069596654052834}]
["ANAMET-M",8150425,"1 1/2\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",1,5.6670883091017572,{"$f":"F1093*(1-Elteq!$F$5)","v":5.6670883091017572}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8150485,"2\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",1,7.097795849432365,{"$f":"F1094*(1-Elteq!$F$5)","v":7.097795849432365}]
["ANAMET-M",8803169,"NPT 1/2\"","Compact fittings for Sealtite, Locknut, stainless steel 304",1,1.9881260625373383,{"$f":"F1095*(1-Elteq!$F$5)","v":1.9881260625373383}]
["ANAMET-M",8803209,"NPT 3/4\"","Compact fittings for Sealtite, Locknut, stainless steel 304",1,2.8892860067715516,{"$f":"F1096*(1-Elteq!$F$5)","v":2.8892860067715516}]
["ANAMET-M",8803269,"NPT 1 \"","Compact fittings for Sealtite, Locknut, stainless steel 304",1,5.1375407130053636,{"$f":"F1097*(1-Elteq!$F$5)","v":5.1375407130053636}]
["ANAMET-M",8803359,"NPT 1 1/4\"","Compact fittings for Sealtite, Locknut, stainless steel 304",1,5.7228301613224302,{"$f":"F1098*(1-Elteq!$F$5)","v":5.7228301613224302}]
["ANAMET-M",8803409,"NPT 1 1/2\"","Compact fittings for Sealtite, Locknut, stainless steel 304",1,7.4694081975701847,{"$f":"F1099*(1-Elteq!$F$5)","v":7.4694081975701847}]
["ANAMET-M",8803509,"NPT 2\"","Compact fittings for Sealtite, Locknut, stainless steel 304",1,11.640756805417215,{"$f":"F1100*(1-Elteq!$F$5)","v":11.640756805417215}]
["ANAMET-M",8100119,"PG 11","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,21.265516622186759,{"$f":"F1101*(1-Elteq!$F$5)","v":21.265516622186759}]
["ANAMET-M",8100129,"PG 11","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,22.696224162517368,{"$f":"F1102*(1-Elteq!$F$5)","v":22.696224162517368}]
["ANAMET-M",8100139,"PG 13,5","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,21.265516622186759,{"$f":"F1103*(1-Elteq!$F$5)","v":21.265516622186759}]
["ANAMET-M",8100149,"PG 13,5","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,22.696224162517368,{"$f":"F1104*(1-Elteq!$F$5)","v":22.696224162517368}]
["ANAMET-M",8100169,"PG 16","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,29.970535877315193,{"$f":"F1105*(1-Elteq!$F$5)","v":29.970535877315193}]
["ANAMET-M",8100219,"PG 21","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,34.467045289782824,{"$f":"F1106*(1-Elteq!$F$5)","v":34.467045289782824}]
["ANAMET-M",8100299,"PG 29","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,42.521742935670076,{"$f":"F1107*(1-Elteq!$F$5)","v":42.521742935670076}]
["ANAMET-M",8100369,"PG 36","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,88.583093487352869,{"$f":"F1108*(1-Elteq!$F$5)","v":88.583093487352869}]
["ANAMET-M",8100429,"PG 42","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,141.95591698864732,{"$f":"F1109*(1-Elteq!$F$5)","v":141.95591698864732}]
["ANAMET-M",8100489,"PG 48","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,216.34341877713544,{"$f":"F1110*(1-Elteq!$F$5)","v":216.34341877713544}]
["ANAMET-M",8109119,"PG 11","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,36.761751539533861,{"$f":"F1111*(1-Elteq!$F$5)","v":36.761751539533861}]
["ANAMET-M",8109129,"PG 11","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,38.192459079864463,{"$f":"F1112*(1-Elteq!$F$5)","v":38.192459079864463}]
["ANAMET-M",8109169,"PG 16","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,51.81205163911558,{"$f":"F1113*(1-Elteq!$F$5)","v":51.81205163911558}]
["ANAMET-M",8109219,"PG 21","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,59.569459406492577,{"$f":"F1114*(1-Elteq!$F$5)","v":59.569459406492577}]
["ANAMET-M",8109299,"PG 29","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,66.79731957777318,{"$f":"F1115*(1-Elteq!$F$5)","v":66.79731957777318}]
["ANAMET-M",8140119,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,23.690287193786038,{"$f":"F1116*(1-Elteq!$F$5)","v":23.690287193786038}]
["ANAMET-M",8140129,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,22.268869962158874,{"$f":"F1117*(1-Elteq!$F$5)","v":22.268869962158874}]
["ANAMET-M",8140169,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,31.401243417645798,{"$f":"F1118*(1-Elteq!$F$5)","v":31.401243417645798}]
["ANAMET-M",8140209,"NPT 3/4\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,36.102139621589231,{"$f":"F1119*(1-Elteq!$F$5)","v":36.102139621589231}]
["ANAMET-M",8140269,"NPT 1 \"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,40.487165329615507,{"$f":"F1120*(1-Elteq!$F$5)","v":40.487165329615507}]
["ANAMET-M",8144119,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 45° elbow, IP 67",1,39.855424337781209,{"$f":"F1121*(1-Elteq!$F$5)","v":39.855424337781209}]
["ANAMET-M",8144129,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 45° elbow, IP 67",1,38.434007106154048,{"$f":"F1122*(1-Elteq!$F$5)","v":38.434007106154048}]
["ANAMET-M",8144169,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 45° elbow, IP 67",1,54.19037066719762,{"$f":"F1123*(1-Elteq!$F$5)","v":54.19037066719762}]
["ANAMET-M",8144209,"NPT 3/4\"","Standard fittings for Sealtite, Stainless steel 304 45° elbow, IP 67",1,62.282229547898666,{"$f":"F1124*(1-Elteq!$F$5)","v":62.282229547898666}]
["ANAMET-M",8149119,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,39.864714646484657,{"$f":"F1125*(1-Elteq!$F$5)","v":39.864714646484657}]
["ANAMET-M",8149129,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,38.434007106154048,{"$f":"F1126*(1-Elteq!$F$5)","v":38.434007106154048}]
["ANAMET-M",8149169,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,54.19037066719762,{"$f":"F1127*(1-Elteq!$F$5)","v":54.19037066719762}]
["ANAMET-M",8149209,"NPT 3/4\"","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,62.282229547898666,{"$f":"F1128*(1-Elteq!$F$5)","v":62.282229547898666}]
["ANAMET-M",8149269,"NPT 1 \"","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",1,69.844540832503313,{"$f":"F1129*(1-Elteq!$F$5)","v":69.844540832503313}]
["ANAMET-M",8150119,"3/8\"","Compact fittings for Sealtite, Ferrule, stainless steel 316",1,13.16436743278228,{"$f":"F1130*(1-Elteq!$F$5)","v":13.16436743278228}]
["ANAMET-M",8150169,"1/2\"","Compact fittings for Sealtite, Ferrule, stainless steel 316",1,17.995327958573945,{"$f":"F1131*(1-Elteq!$F$5)","v":17.995327958573945}]
["ANAMET-M",8150219,"3/4\"","Compact fittings for Sealtite, Ferrule, stainless steel 316",1,23.22577175861376,{"$f":"F1132*(1-Elteq!$F$5)","v":23.22577175861376}]
["ANAMET-M",8150299,"1\"","Compact fittings for Sealtite, Ferrule, stainless steel 316",1,29.868342481577294,{"$f":"F1133*(1-Elteq!$F$5)","v":29.868342481577294}]
["ANAMET-M",7121149,"M20 x 1,5","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,31.605630209121603,{"$f":"F1134*(1-Elteq!$F$5)","v":31.605630209121603}]
["ANAMET-M",7121159,"M16 x 1,5","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,23.513771328420571,{"$f":"F1135*(1-Elteq!$F$5)","v":23.513771328420571}]
["ANAMET-M",7121169,"M16 x 1,5","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,23.513771328420571,{"$f":"F1136*(1-Elteq!$F$5)","v":23.513771328420571}]
["ANAMET-M",7121179,"M20 x 1,5","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,31.605630209121603,{"$f":"F1137*(1-Elteq!$F$5)","v":31.605630209121603}]
["ANAMET-M",7121209,"M20 x 1,5","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,31.605630209121603,{"$f":"F1138*(1-Elteq!$F$5)","v":31.605630209121603}]
["ANAMET-M",7121259,"M25 x 1,5","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,37.62575024895429,{"$f":"F1139*(1-Elteq!$F$5)","v":37.62575024895429}]
["ANAMET-M",7121329,"M32 x 1,5","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,46.888188026289463,{"$f":"F1140*(1-Elteq!$F$5)","v":46.888188026289463}]
["ANAMET-M",7121409,"M40 x 1,5","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,69.240670766779346,{"$f":"F1141*(1-Elteq!$F$5)","v":69.240670766779346}]
["ANAMET-M",7121509,"M50 x 1,5","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,103.72629667396906,{"$f":"F1142*(1-Elteq!$F$5)","v":103.72629667396906}]
["ANAMET-M",7121639,"M63 x 1,5","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,147.95745641107308,{"$f":"F1143*(1-Elteq!$F$5)","v":147.95745641107308}]
["ANAMET-M",7125169,"M16 x 1,5","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,48.922765632344024,{"$f":"F1144*(1-Elteq!$F$5)","v":48.922765632344024}]
["ANAMET-M",7125179,"M20 x 1,5","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,50.4277956423022,{"$f":"F1145*(1-Elteq!$F$5)","v":50.4277956423022}]
["ANAMET-M",7125209,"M20 x 1,5","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,55.537465429197219,{"$f":"F1146*(1-Elteq!$F$5)","v":55.537465429197219}]
["ANAMET-M",7125259,"M25 x 1,5","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,71.498215781716596,{"$f":"F1147*(1-Elteq!$F$5)","v":71.498215781716596}]
["ANAMET-M",7125329,"M32 x 1,5","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,107.31235583349903,{"$f":"F1148*(1-Elteq!$F$5)","v":107.31235583349903}]
["ANAMET-M",7125409,"M40 x 1,5","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,137.71953621987618,{"$f":"F1149*(1-Elteq!$F$5)","v":137.71953621987618}]
["ANAMET-M",7125509,"M50 x 1,5","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,197.15893130452051,{"$f":"F1150*(1-Elteq!$F$5)","v":197.15893130452051}]
["ANAMET-M",7125639,"M63 x 1,5","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,282.94564187213626,{"$f":"F1151*(1-Elteq!$F$5)","v":282.94564187213626}]
["ANAMET-M",7141129,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,23.513771328420571,{"$f":"F1152*(1-Elteq!$F$5)","v":23.513771328420571}]
["ANAMET-M",7141169,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,31.605630209121603,{"$f":"F1153*(1-Elteq!$F$5)","v":31.605630209121603}]
["ANAMET-M",7141209,"NPT 3/4\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,37.62575024895429,{"$f":"F1154*(1-Elteq!$F$5)","v":37.62575024895429}]
["ANAMET-M",7141269,"NPT 1\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,46.888188026289463,{"$f":"F1155*(1-Elteq!$F$5)","v":46.888188026289463}]
["ANAMET-M",7141359,"NPT 1.1/4\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,69.240670766779346,{"$f":"F1156*(1-Elteq!$F$5)","v":69.240670766779346}]
["ANAMET-M",7141409,"NPT 1.1/2\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,103.72629667396906,{"$f":"F1157*(1-Elteq!$F$5)","v":103.72629667396906}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},7141509,"NPT 2\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,147.95745641107308,{"$f":"F1158*(1-Elteq!$F$5)","v":147.95745641107308}]
["ANAMET-M",7145129,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,48.922765632344024,{"$f":"F1159*(1-Elteq!$F$5)","v":48.922765632344024}]
["ANAMET-M",7145169,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,55.537465429197219,{"$f":"F1160*(1-Elteq!$F$5)","v":55.537465429197219}]
["ANAMET-M",7145209,"NPT 3/4\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,71.498215781716596,{"$f":"F1161*(1-Elteq!$F$5)","v":71.498215781716596}]
["ANAMET-M",7145269,"NPT 1\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,107.31235583349903,{"$f":"F1162*(1-Elteq!$F$5)","v":107.31235583349903}]
["ANAMET-M",7145359,"NPT 1.1/4\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,137.71953621987618,{"$f":"F1163*(1-Elteq!$F$5)","v":137.71953621987618}]
["ANAMET-M",7145409,"NPT 1.1/2\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,197.15893130452051,{"$f":"F1164*(1-Elteq!$F$5)","v":197.15893130452051}]
["ANAMET-M",7145509,"NPT 2\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,282.94564187213626,{"$f":"F1165*(1-Elteq!$F$5)","v":282.94564187213626}]
["ANAMET-M",71411292,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,26.626024744074815,{"$f":"F1166*(1-Elteq!$F$5)","v":26.626024744074815}]
["ANAMET-M",71411692,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,34.717883624775851,{"$f":"F1167*(1-Elteq!$F$5)","v":34.717883624775851}]
["ANAMET-M",71412092,"NPT 3/4\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,40.793745516829205,{"$f":"F1168*(1-Elteq!$F$5)","v":40.793745516829205}]
["ANAMET-M",71412692,"NPT 1\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,51.877083800039699,{"$f":"F1169*(1-Elteq!$F$5)","v":51.877083800039699}]
["ANAMET-M",71413592,"NPT 1.1/4\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,75.911112415853211,{"$f":"F1170*(1-Elteq!$F$5)","v":75.911112415853211}]
["ANAMET-M",71414092,"NPT 1.1/2\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,112.91441198167665,{"$f":"F1171*(1-Elteq!$F$5)","v":112.91441198167665}]
["ANAMET-M",71415092,"NPT 2\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,162.89627280621349,{"$f":"F1172*(1-Elteq!$F$5)","v":162.89627280621349}]
["ANAMET-M",71451292,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,52.02572873929482,{"$f":"F1173*(1-Elteq!$F$5)","v":52.02572873929482}]
["ANAMET-M",71451692,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,58.649718844851463,{"$f":"F1174*(1-Elteq!$F$5)","v":58.649718844851463}]
["ANAMET-M",71452092,"NPT 3/4\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,74.656920740888069,{"$f":"F1175*(1-Elteq!$F$5)","v":74.656920740888069}]
["ANAMET-M",71452692,"NPT 1\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,112.30125160724926,{"$f":"F1176*(1-Elteq!$F$5)","v":112.30125160724926}]
["ANAMET-M",71453592,"NPT 1.1/4\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,144.3806875602466,{"$f":"F1177*(1-Elteq!$F$5)","v":144.3806875602466}]
["ANAMET-M",71454092,"NPT 1.1/2\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,206.34704661222813,{"$f":"F1178*(1-Elteq!$F$5)","v":206.34704661222813}]
["ANAMET-M",71455092,"NPT 2\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,297.88445826727661,{"$f":"F1179*(1-Elteq!$F$5)","v":297.88445826727661}]
["ANAMET-M",8101169,"PG 16","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,34.671432081258622,{"$f":"F1180*(1-Elteq!$F$5)","v":34.671432081258622}]
["ANAMET-M",8101219,"PG 21","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,51.626245465046672,{"$f":"F1181*(1-Elteq!$F$5)","v":51.626245465046672}]
["ANAMET-M",8101299,"PG 29","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,68.961961505675987,{"$f":"F1182*(1-Elteq!$F$5)","v":68.961961505675987}]
["ANAMET-M",8121169,"M16 x 1,5","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,30.407180386377131,{"$f":"F1183*(1-Elteq!$F$5)","v":30.407180386377131}]
["ANAMET-M",8121209,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,34.671432081258622,{"$f":"F1184*(1-Elteq!$F$5)","v":34.671432081258622}]
["ANAMET-M",8121259,"M25 x 1,5","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,51.626245465046672,{"$f":"F1185*(1-Elteq!$F$5)","v":51.626245465046672}]
["ANAMET-M",8121329,"M32 x 1,5","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,68.961961505675987,{"$f":"F1186*(1-Elteq!$F$5)","v":68.961961505675987}]
["ANAMET-M",8141129,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,30.407180386377131,{"$f":"F1187*(1-Elteq!$F$5)","v":30.407180386377131}]
["ANAMET-M",8141169,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,34.671432081258622,{"$f":"F1188*(1-Elteq!$F$5)","v":34.671432081258622}]
["ANAMET-M",8141209,"NPT 3/4\"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,51.626245465046672,{"$f":"F1189*(1-Elteq!$F$5)","v":51.626245465046672}]
["ANAMET-M",8141269,"NPT 1 \"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,68.961961505675987,{"$f":"F1190*(1-Elteq!$F$5)","v":68.961961505675987}]
["ANAMET-M",8145129,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,68.738994096793277,{"$f":"F1191*(1-Elteq!$F$5)","v":68.738994096793277}]
["ANAMET-M",8145169,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,79.617945588527974,{"$f":"F1192*(1-Elteq!$F$5)","v":79.617945588527974}]
["ANAMET-M",8145209,"NPT 3/4\"","Standard fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",1,95.216373901612954,{"$f":"F1193*(1-Elteq!$F$5)","v":95.216373901612954}]
["ANAMET-M",8150115,"3/8\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",1,3.1679952678749173,{"$f":"F1194*(1-Elteq!$F$5)","v":3.1679952678749173}]
["ANAMET-M",8150119,"3/8\"","Compact fittings for Sealtite, Ferrule, stainless steel 316",1,13.16436743278228,{"$f":"F1195*(1-Elteq!$F$5)","v":13.16436743278228}]
["ANAMET-M",8150165,"1/2\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",1,3.7904459510057658,{"$f":"F1196*(1-Elteq!$F$5)","v":3.7904459510057658}]
["ANAMET-M",8150169,"1/2\"","Compact fittings for Sealtite, Ferrule, stainless steel 316",1,17.995327958573945,{"$f":"F1197*(1-Elteq!$F$5)","v":17.995327958573945}]
["ANAMET-M",8150215,"3/4\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",1,4.4407675602469512,{"$f":"F1198*(1-Elteq!$F$5)","v":4.4407675602469512}]
["ANAMET-M",8150219,"3/4\"","Compact fittings for Sealtite, Ferrule, stainless steel 316",1,23.22577175861376,{"$f":"F1199*(1-Elteq!$F$5)","v":23.22577175861376}]
["ANAMET-M",8150295,"1\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",1,5.0632182433777997,{"$f":"F1200*(1-Elteq!$F$5)","v":5.0632182433777997}]
["ANAMET-M",8150299,"1\"","Compact fittings for Sealtite, Ferrule, stainless steel 316",1,29.868342481577294,{"$f":"F1201*(1-Elteq!$F$5)","v":29.868342481577294}]
["ANAMET-M",8150365,"1 1/4\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",1,5.4069596654052834,{"$f":"F1202*(1-Elteq!$F$5)","v":5.4069596654052834}]
["ANAMET-M",8150425,"1 1/2\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",1,5.6670883091017572,{"$f":"F1203*(1-Elteq!$F$5)","v":5.6670883091017572}]
["ANAMET-M",8150485,"2\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",1,7.097795849432365,{"$f":"F1204*(1-Elteq!$F$5)","v":7.097795849432365}]
["ANAMET-M",8803169,"NPT 1/2\"","Compact fittings for Sealtite, Locknut, stainless steel 304",1,1.9881260625373383,{"$f":"F1205*(1-Elteq!$F$5)","v":1.9881260625373383}]
["ANAMET-M",8803209,"NPT 3/4\"","Compact fittings for Sealtite, Locknut, stainless steel 304",1,2.8892860067715516,{"$f":"F1206*(1-Elteq!$F$5)","v":2.8892860067715516}]
["ANAMET-M",8803269,"NPT 1 \"","Compact fittings for Sealtite, Locknut, stainless steel 304",1,5.1375407130053636,{"$f":"F1207*(1-Elteq!$F$5)","v":5.1375407130053636}]
["ANAMET-M",8803359,"NPT 1 1/4\"","Compact fittings for Sealtite, Locknut, stainless steel 304",1,5.7228301613224302,{"$f":"F1208*(1-Elteq!$F$5)","v":5.7228301613224302}]
["ANAMET-M",8803409,"NPT 1 1/2\"","Compact fittings for Sealtite, Locknut, stainless steel 304",1,7.4694081975701847,{"$f":"F1209*(1-Elteq!$F$5)","v":7.4694081975701847}]
["ANAMET-M",8803509,"NPT 2\"","Compact fittings for Sealtite, Locknut, stainless steel 304",1,11.640756805417215,{"$f":"F1210*(1-Elteq!$F$5)","v":11.640756805417215}]
["ANAMET-M",8189161,"M16 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",1,16.165137143995175,{"$f":"F1211*(1-Elteq!$F$5)","v":16.165137143995175}]
["ANAMET-M",8189201,"M20 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",1,20.624485321649018,{"$f":"F1212*(1-Elteq!$F$5)","v":20.624485321649018}]
["ANAMET-M",8189251,"M25 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",1,26.087186839274974,{"$f":"F1213*(1-Elteq!$F$5)","v":26.087186839274974}]
["ANAMET-M",8189321,"M32 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",1,45.485351412069186,{"$f":"F1214*(1-Elteq!$F$5)","v":45.485351412069186}]
["ANAMET-M",8192129,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67","1",58.696170388368699,{"$f":"F1215*(1-Elteq!$F$5)","v":58.696170388368699}]
["ANAMET-M",8192169,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67","1",77.035239768970129,{"$f":"F1216*(1-Elteq!$F$5)","v":77.035239768970129}]
["ANAMET-M",8195129,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67","1",58.696170388368699,{"$f":"F1217*(1-Elteq!$F$5)","v":58.696170388368699}]
["ANAMET-M",8195169,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67","1",77.035239768970129,{"$f":"F1218*(1-Elteq!$F$5)","v":77.035239768970129}]
["ANAMET-M",8320169,"M 16 x 1,5","Food grade fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,49.136442732523271,{"$f":"F1219*(1-Elteq!$F$5)","v":49.136442732523271}]
["ANAMET-M",8320209,"M 20 x 1,5","Food grade fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,49.136442732523271,{"$f":"F1220*(1-Elteq!$F$5)","v":49.136442732523271}]
["ANAMET-M",8320259,"M 25 x 1,5","Food grade fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,66.481449081856027,{"$f":"F1221*(1-Elteq!$F$5)","v":66.481449081856027}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8320329,"M 32 x 1,5","Food grade fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,98.337917625970647,{"$f":"F1222*(1-Elteq!$F$5)","v":98.337917625970647}]
["ANAMET-M",8382209,"NPT 3/4\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67",1,118.84162893447488,{"$f":"F1223*(1-Elteq!$F$5)","v":118.84162893447488}]
["ANAMET-M",8382269,"NPT 1\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67",1,182.52112091137175,{"$f":"F1224*(1-Elteq!$F$5)","v":182.52112091137175}]
["ANAMET-M",8385209,"NPT 3/4\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67",1,118.84162893447488,{"$f":"F1225*(1-Elteq!$F$5)","v":118.84162893447488}]
["ANAMET-M",8385269,"NPT 1\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67",1,182.52112091137175,{"$f":"F1226*(1-Elteq!$F$5)","v":182.52112091137175}]
["ANAMET-M",2950120,"M 16 x 1,5","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,7.3207632583150577,{"$f":"F1227*(1-Elteq!$F$5)","v":7.3207632583150577}]
["ANAMET-M",2950160,"M 20 x 1,5","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,7.8596011631148972,{"$f":"F1228*(1-Elteq!$F$5)","v":7.8596011631148972}]
["ANAMET-M",2950200,"M 25 x 1,5","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,11.61288587930688,{"$f":"F1229*(1-Elteq!$F$5)","v":11.61288587930688}]
["ANAMET-M",2950260,"M 32 x 1,5","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,16.629652579167452,{"$f":"F1230*(1-Elteq!$F$5)","v":16.629652579167452}]
["ANAMET-M",2954120,"M16 x 1,5","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,12.727722923720341,{"$f":"F1231*(1-Elteq!$F$5)","v":12.727722923720341}]
["ANAMET-M",2954160,"M20 x 1,5","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,15.050300099581717,{"$f":"F1232*(1-Elteq!$F$5)","v":15.050300099581717}]
["ANAMET-M",2954200,"M25 x 1,5","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,22.668353236407029,{"$f":"F1233*(1-Elteq!$F$5)","v":22.668353236407029}]
["ANAMET-M",2954260,"M32 x 1,5","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,41.806389165504768,{"$f":"F1234*(1-Elteq!$F$5)","v":41.806389165504768}]
["ANAMET-M",2959120,"M16 x 1,5","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,12.727722923720341,{"$f":"F1235*(1-Elteq!$F$5)","v":12.727722923720341}]
["ANAMET-M",2959160,"M20 x 1,5","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,15.050300099581717,{"$f":"F1236*(1-Elteq!$F$5)","v":15.050300099581717}]
["ANAMET-M",2959200,"M25 x 1,5","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,22.668353236407029,{"$f":"F1237*(1-Elteq!$F$5)","v":22.668353236407029}]
["ANAMET-M",2959260,"M32 x 1,5","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,41.806389165504768,{"$f":"F1238*(1-Elteq!$F$5)","v":41.806389165504768}]
["ANAMET-M",2980120,"NPT 1/2\"","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,7.8596011631148972,{"$f":"F1239*(1-Elteq!$F$5)","v":7.8596011631148972}]
["ANAMET-M",2980160,"NPT 1/2\"","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,7.8596011631148972,{"$f":"F1240*(1-Elteq!$F$5)","v":7.8596011631148972}]
["ANAMET-M",2980200,"NPT 3/4\"","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,11.42707970523797,{"$f":"F1241*(1-Elteq!$F$5)","v":11.42707970523797}]
["ANAMET-M",2980260,"NPT 1\"","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,17.744489623580915,{"$f":"F1242*(1-Elteq!$F$5)","v":17.744489623580915}]
["ANAMET-M",2980350,"NPT 1 1/4\"","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,29.264472415853337,{"$f":"F1243*(1-Elteq!$F$5)","v":29.264472415853337}]
["ANAMET-M",2984120,"NPT 1/2\"","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,12.913529097789251,{"$f":"F1244*(1-Elteq!$F$5)","v":12.913529097789251}]
["ANAMET-M",2984160,"NPT 1/2\"","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,12.913529097789251,{"$f":"F1245*(1-Elteq!$F$5)","v":12.913529097789251}]
["ANAMET-M",2984200,"NPT 3/4\"","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,19.602551364270013,{"$f":"F1246*(1-Elteq!$F$5)","v":19.602551364270013}]
["ANAMET-M",2984260,"NPT 1\"","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,37.161234813782016,{"$f":"F1247*(1-Elteq!$F$5)","v":37.161234813782016}]
["ANAMET-M",2984350,"NPT 1 1/4\"","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,60.201200398326868,{"$f":"F1248*(1-Elteq!$F$5)","v":60.201200398326868}]
["ANAMET-M",2986120,"NPT 1/2\"","Steel fittings for Sealtite, Straight fixed with female thread, IP 67",1,9.4761148775144139,{"$f":"F1249*(1-Elteq!$F$5)","v":9.4761148775144139}]
["ANAMET-M",2986160,"NPT 1/2\"","Steel fittings for Sealtite, Straight fixed with female thread, IP 67",1,9.8477272256522355,{"$f":"F1250*(1-Elteq!$F$5)","v":9.8477272256522355}]
["ANAMET-M",2986200,"NPT 3/4\"","Steel fittings for Sealtite, Straight fixed with female thread, IP 67",1,13.470947619995981,{"$f":"F1251*(1-Elteq!$F$5)","v":13.470947619995981}]
["ANAMET-M",2986260,"NPT 1\"","Steel fittings for Sealtite, Straight fixed with female thread, IP 67",1,18.580617406891008,{"$f":"F1252*(1-Elteq!$F$5)","v":18.580617406891008}]
["ANAMET-M",2990110,"PG 11","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,7.3207632583150577,{"$f":"F1253*(1-Elteq!$F$5)","v":7.3207632583150577}]
["ANAMET-M",2990130,"PG 13,5","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,7.3207632583150577,{"$f":"F1254*(1-Elteq!$F$5)","v":7.3207632583150577}]
["ANAMET-M",2990160,"PG 16","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,7.8596011631148972,{"$f":"F1255*(1-Elteq!$F$5)","v":7.8596011631148972}]
["ANAMET-M",2990200,"PG 21","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,11.61288587930688,{"$f":"F1256*(1-Elteq!$F$5)","v":11.61288587930688}]
["ANAMET-M",2990260,"PG 29","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,17.372877275443091,{"$f":"F1257*(1-Elteq!$F$5)","v":17.372877275443091}]
["ANAMET-M",2990350,"PG 36","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,31.679952678749167,{"$f":"F1258*(1-Elteq!$F$5)","v":31.679952678749167}]
["ANAMET-M",2994110,"PG 11","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,13.378044532961527,{"$f":"F1259*(1-Elteq!$F$5)","v":13.378044532961527}]
["ANAMET-M",2994130,"PG 13,5","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,13.378044532961527,{"$f":"F1260*(1-Elteq!$F$5)","v":13.378044532961527}]
["ANAMET-M",2994160,"PG 16","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,15.514815534753993,{"$f":"F1261*(1-Elteq!$F$5)","v":15.514815534753993}]
["ANAMET-M",2994200,"PG 21","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,20.345776060545653,{"$f":"F1262*(1-Elteq!$F$5)","v":20.345776060545653}]
["ANAMET-M",2994260,"PG 29","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,36.139300856403004,{"$f":"F1263*(1-Elteq!$F$5)","v":36.139300856403004}]
["ANAMET-M",2994350,"PG 36","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,53.047662696673832,{"$f":"F1264*(1-Elteq!$F$5)","v":53.047662696673832}]
["ANAMET-M",2999110,"PG 11","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,13.378044532961527,{"$f":"F1265*(1-Elteq!$F$5)","v":13.378044532961527}]
["ANAMET-M",2999130,"PG 13,5","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,13.378044532961527,{"$f":"F1266*(1-Elteq!$F$5)","v":13.378044532961527}]
["ANAMET-M",2999160,"PG 16","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,15.514815534753993,{"$f":"F1267*(1-Elteq!$F$5)","v":15.514815534753993}]
["ANAMET-M",2999200,"PG 21","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,20.345776060545653,{"$f":"F1268*(1-Elteq!$F$5)","v":20.345776060545653}]
["ANAMET-M",2999260,"PG 29","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,36.139300856403004,{"$f":"F1269*(1-Elteq!$F$5)","v":36.139300856403004}]
["ANAMET-M",2972120,"-","Steel fittings for Sealtite, Ferrule, galvanised steel",1,2.2018031627165846,{"$f":"F1270*(1-Elteq!$F$5)","v":2.2018031627165846}]
["ANAMET-M",2972160,"-","Steel fittings for Sealtite, Ferrule, galvanised steel",1,2.2018031627165846,{"$f":"F1271*(1-Elteq!$F$5)","v":2.2018031627165846}]
["ANAMET-M",2972200,"-","Steel fittings for Sealtite, Ferrule, galvanised steel",1,2.4712221151165039,{"$f":"F1272*(1-Elteq!$F$5)","v":2.4712221151165039}]
["ANAMET-M",2972260,"-","Steel fittings for Sealtite, Ferrule, galvanised steel",1,3.59534946823341,{"$f":"F1273*(1-Elteq!$F$5)","v":3.59534946823341}]
["ANAMET-M",2972350,"-","Steel fittings for Sealtite, Ferrule, galvanised steel",1,8.4263099940250736,{"$f":"F1274*(1-Elteq!$F$5)","v":8.4263099940250736}]
["ANAMET-M",2972400,"-","Steel fittings for Sealtite, Ferrule, galvanised steel",1,10.776758095996785,{"$f":"F1275*(1-Elteq!$F$5)","v":10.776758095996785}]
["ANAMET-M",2972500,"-","Steel fittings for Sealtite, Ferrule, galvanised steel",1,14.957397012547263,{"$f":"F1276*(1-Elteq!$F$5)","v":14.957397012547263}]
["ANAMET-M",2972630,"-","Steel fittings for Sealtite, Ferrule, galvanised steel",1,63.452808444532792,{"$f":"F1277*(1-Elteq!$F$5)","v":63.452808444532792}]
["ANAMET-M",2972750,"-","Steel fittings for Sealtite, Ferrule, galvanised steel",1,85.842452419836462,{"$f":"F1278*(1-Elteq!$F$5)","v":85.842452419836462}]
["ANAMET-M",2974160,"-","Steel fittings for Sealtite, Locknut, galvanised steel",1,0.5109669786895028,{"$f":"F1279*(1-Elteq!$F$5)","v":0.5109669786895028}]
["ANAMET-M",2974200,"-","Steel fittings for Sealtite, Locknut, galvanised steel",1,0.85470840071698639,{"$f":"F1280*(1-Elteq!$F$5)","v":0.85470840071698639}]
["ANAMET-M",2974260,"-","Steel fittings for Sealtite, Locknut, galvanised steel",1,1.4771590838478352,{"$f":"F1281*(1-Elteq!$F$5)","v":1.4771590838478352}]
["ANAMET-M",2974350,"-","Steel fittings for Sealtite, Locknut, galvanised steel",1,1.7837392710615367,{"$f":"F1282*(1-Elteq!$F$5)","v":1.7837392710615367}]
["ANAMET-M",2974400,"-","Steel fittings for Sealtite, Locknut, galvanised steel",1,2.7127701414060872,{"$f":"F1283*(1-Elteq!$F$5)","v":2.7127701414060872}]
["ANAMET-M",2974500,"-","Steel fittings for Sealtite, Locknut, galvanised steel",1,4.0784455208125756,{"$f":"F1284*(1-Elteq!$F$5)","v":4.0784455208125756}]
["ANAMET-M",2982120,"22/25 mm","Steel fittings for Sealtite, Straight box connector, IP 67",1,12.356110575582521,{"$f":"F1285*(1-Elteq!$F$5)","v":12.356110575582521}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},2982160,"22/25 mm","Steel fittings for Sealtite, Straight box connector, IP 67",1,12.356110575582521,{"$f":"F1286*(1-Elteq!$F$5)","v":12.356110575582521}]
["ANAMET-M",2982200,"28/31 mm","Steel fittings for Sealtite, Straight box connector, IP 67",1,17.558683449512003,{"$f":"F1287*(1-Elteq!$F$5)","v":17.558683449512003}]
["ANAMET-M",2982260,"34/37 mm","Steel fittings for Sealtite, Straight box connector, IP 67",1,27.313507588129781,{"$f":"F1288*(1-Elteq!$F$5)","v":27.313507588129781}]
["ANAMET-M",2982350,"43/47 mm","Steel fittings for Sealtite, Straight box connector, IP 67",1,42.549613861780408,{"$f":"F1289*(1-Elteq!$F$5)","v":42.549613861780408}]
["ANAMET-M",2988120,"22/25 mm","Steel fittings for Sealtite, 90° elbow box connector, IP 67",1,21.646419279028024,{"$f":"F1290*(1-Elteq!$F$5)","v":21.646419279028024}]
["ANAMET-M",2988160,"22/25 mm","Steel fittings for Sealtite, 90° elbow box connector, IP 67",1,21.646419279028024,{"$f":"F1291*(1-Elteq!$F$5)","v":21.646419279028024}]
["ANAMET-M",2988200,"28/31 mm","Steel fittings for Sealtite, 90° elbow box connector, IP 67",1,34.467045289782824,{"$f":"F1292*(1-Elteq!$F$5)","v":34.467045289782824}]
["ANAMET-M",2988260,"34/37 mm","Steel fittings for Sealtite, 90° elbow box connector, IP 67",1,46.45154351722752,{"$f":"F1293*(1-Elteq!$F$5)","v":46.45154351722752}]
["ANAMET-M",2989120,"NPT 1/2\"","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,12.913529097789251,{"$f":"F1294*(1-Elteq!$F$5)","v":12.913529097789251}]
["ANAMET-M",2989160,"NPT 1/2\"","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,12.913529097789251,{"$f":"F1295*(1-Elteq!$F$5)","v":12.913529097789251}]
["ANAMET-M",2989200,"NPT 3/4\"","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,19.602551364270013,{"$f":"F1296*(1-Elteq!$F$5)","v":19.602551364270013}]
["ANAMET-M",2989260,"NPT 1\"","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,37.161234813782016,{"$f":"F1297*(1-Elteq!$F$5)","v":37.161234813782016}]
["ANAMET-M",2989350,"NPT 1 1/4\"","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,60.201200398326868,{"$f":"F1298*(1-Elteq!$F$5)","v":60.201200398326868}]
["ANAMET-M",8103032,"PG11","Special fittings for Sealtite, Power connector adapter, IP 67",1,12.179594710217057,{"$f":"F1299*(1-Elteq!$F$5)","v":12.179594710217057}]
["ANAMET-M",8103036,"PG11","Special fittings for Sealtite, Power connector adapter, IP 67",1,13.071464345747824,{"$f":"F1300*(1-Elteq!$F$5)","v":13.071464345747824}]
["ANAMET-M",8103037,"PG11","Special fittings for Sealtite, Power connector adapter, IP 67",1,15.189654730133402,{"$f":"F1301*(1-Elteq!$F$5)","v":15.189654730133402}]
["ANAMET-M",8103041,"PG11","Special fittings for Sealtite, Power connector adapter, IP 67",1,10.758177478589893,{"$f":"F1302*(1-Elteq!$F$5)","v":10.758177478589893}]
["ANAMET-M",8103045,"PG11","Special fittings for Sealtite, Power connector adapter, IP 68",1,13.322302680740853,{"$f":"F1303*(1-Elteq!$F$5)","v":13.322302680740853}]
["ANAMET-M",8103046,"PG11","Special fittings for Sealtite, Power connector adapter, IP 40",1,14.214172316271622,{"$f":"F1304*(1-Elteq!$F$5)","v":14.214172316271622}]
["ANAMET-M",8103047,"PG11","Special fittings for Sealtite, Power connector adapter, IP 40",1,13.545270089623546,{"$f":"F1305*(1-Elteq!$F$5)","v":13.545270089623546}]
["ANAMET-M",8123231,"M24 x 1","Special fittings for Sealtite, Power connector adapter, IP 67",1,10.758177478589893,{"$f":"F1306*(1-Elteq!$F$5)","v":10.758177478589893}]
["ANAMET-M",8123235,"M24 x 1","Special fittings for Sealtite, Power connector adapter, IP 68",1,13.322302680740853,{"$f":"F1307*(1-Elteq!$F$5)","v":13.322302680740853}]
["ANAMET-M",8123236,"M24 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",1,14.214172316271622,{"$f":"F1308*(1-Elteq!$F$5)","v":14.214172316271622}]
["ANAMET-M",8123237,"M24 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",1,13.545270089623546,{"$f":"F1309*(1-Elteq!$F$5)","v":13.545270089623546}]
["ANAMET-M",8123271,"M25 x 1","Special fittings for Sealtite, Power connector adapter, IP 67",1,13.173657741485725,{"$f":"F1310*(1-Elteq!$F$5)","v":13.173657741485725}]
["ANAMET-M",8123275,"M25 x 1","Special fittings for Sealtite, Power connector adapter, IP 68",1,15.960750352519376,{"$f":"F1311*(1-Elteq!$F$5)","v":15.960750352519376}]
["ANAMET-M",8123276,"M25 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",1,16.629652579167452,{"$f":"F1312*(1-Elteq!$F$5)","v":16.629652579167452}]
["ANAMET-M",8123277,"M25 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",1,16.79687813582947,{"$f":"F1313*(1-Elteq!$F$5)","v":16.79687813582947}]
["ANAMET-M",8123291,"M25 x 1","Special fittings for Sealtite, Power connector adapter, IP 67",1,15.273267508464411,{"$f":"F1314*(1-Elteq!$F$5)","v":15.273267508464411}]
["ANAMET-M",8123295,"M25 x 1","Special fittings for Sealtite, Power connector adapter, IP 68",1,18.060360119498061,{"$f":"F1315*(1-Elteq!$F$5)","v":18.060360119498061}]
["ANAMET-M",8123296,"M25 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",1,19.732615686118248,{"$f":"F1316*(1-Elteq!$F$5)","v":19.732615686118248}]
["ANAMET-M",8123297,"M25 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",1,20.735969026090366,{"$f":"F1317*(1-Elteq!$F$5)","v":20.735969026090366}]
["ANAMET-M",8123381,"M40 x 1","Special fittings for Sealtite, Power connector adapter, IP 67",1,23.039965584544852,{"$f":"F1318*(1-Elteq!$F$5)","v":23.039965584544852}]
["ANAMET-M",8123386,"M40 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",1,29.840471555466959,{"$f":"F1319*(1-Elteq!$F$5)","v":29.840471555466959}]
["ANAMET-M",8123387,"M40 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",1,32.516080462059264,{"$f":"F1320*(1-Elteq!$F$5)","v":32.516080462059264}]
["ANAMET-M",8123421,"M40 x 1","Special fittings for Sealtite, Power connector adapter, IP 67",1,50.065473602867826,{"$f":"F1321*(1-Elteq!$F$5)","v":50.065473602867826}]
["ANAMET-M",8123426,"M40 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",1,54.301854371638974,{"$f":"F1322*(1-Elteq!$F$5)","v":54.301854371638974}]
["ANAMET-M",8123427,"M40 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",1,60.201200398326868,{"$f":"F1323*(1-Elteq!$F$5)","v":60.201200398326868}]
["ANAMET-M",8175120,"13 mm","Special fittings for Sealtite, Clamping ring for mounting fittings",1,2.0067066799442288,{"$f":"F1324*(1-Elteq!$F$5)","v":2.0067066799442288}]
["ANAMET-M",8175160,"16 mm","Special fittings for Sealtite, Clamping ring for mounting fittings",1,2.5641252021509588,{"$f":"F1325*(1-Elteq!$F$5)","v":2.5641252021509588}]
["ANAMET-M",8175200,"22 mm","Special fittings for Sealtite, Clamping ring for mounting fittings",1,3.0658018721370164,{"$f":"F1326*(1-Elteq!$F$5)","v":3.0658018721370164}]
["ANAMET-M",8175260,"25 mm","Special fittings for Sealtite, Clamping ring for mounting fittings",1,4.0691552121091306,{"$f":"F1327*(1-Elteq!$F$5)","v":4.0691552121091306}]
["ANAMET-M",8175350,"35 mm","Special fittings for Sealtite, Clamping ring for mounting fittings",1,4.738057438757207,{"$f":"F1328*(1-Elteq!$F$5)","v":4.738057438757207}]
["ANAMET-M",8175400,"38 mm","Special fittings for Sealtite, Clamping ring for mounting fittings",1,8.1383104242182611,{"$f":"F1329*(1-Elteq!$F$5)","v":8.1383104242182611}]
["ANAMET-M",8175500,"51 mm","Special fittings for Sealtite, Clamping ring for mounting fittings",1,14.938816395140369,{"$f":"F1330*(1-Elteq!$F$5)","v":14.938816395140369}]
["ANAMET-M",8123221,"M25 x 1","Special fittings for Sealtite, Power connector adapter, IP 67",1,10.758177478589893,{"$f":"F1331*(1-Elteq!$F$5)","v":10.758177478589893}]
["ANAMET-M",8123226,"M25 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",1,14.214172316271622,{"$f":"F1332*(1-Elteq!$F$5)","v":14.214172316271622}]
["ANAMET-M",8123227,"M25 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",1,13.545270089623546,{"$f":"F1333*(1-Elteq!$F$5)","v":13.545270089623546}]
["ANAMET-M",8123261,"M24 x 1","Special fittings for Sealtite, Power connector adapter, IP 67",1,10.758177478589893,{"$f":"F1334*(1-Elteq!$F$5)","v":10.758177478589893}]
["ANAMET-M",8123266,"M24 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",1,14.214172316271622,{"$f":"F1335*(1-Elteq!$F$5)","v":14.214172316271622}]
["ANAMET-M",8123267,"M24 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",1,14.38139787293364,{"$f":"F1336*(1-Elteq!$F$5)","v":14.38139787293364}]
["ANAMET-M",8833080,"M8 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 65",1,16.583201035650223,{"$f":"F1337*(1-Elteq!$F$5)","v":16.583201035650223}]
["ANAMET-M",8833086,"M8 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",1,17.47507067118099,{"$f":"F1338*(1-Elteq!$F$5)","v":17.47507067118099}]
["ANAMET-M",8833087,"M8 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",1,17.47507067118099,{"$f":"F1339*(1-Elteq!$F$5)","v":17.47507067118099}]
["ANAMET-M",8833100,"M8 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 65",1,16.583201035650223,{"$f":"F1340*(1-Elteq!$F$5)","v":16.583201035650223}]
["ANAMET-M",8833106,"M8 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",1,17.47507067118099,{"$f":"F1341*(1-Elteq!$F$5)","v":17.47507067118099}]
["ANAMET-M",8833107,"M8 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",1,19.37029364668388,{"$f":"F1342*(1-Elteq!$F$5)","v":19.37029364668388}]
["ANAMET-M",8833120,"M12 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 65",1,16.583201035650223,{"$f":"F1343*(1-Elteq!$F$5)","v":16.583201035650223}]
["ANAMET-M",8833126,"M12 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",1,17.47507067118099,{"$f":"F1344*(1-Elteq!$F$5)","v":17.47507067118099}]
["ANAMET-M",8833127,"M12 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",1,17.47507067118099,{"$f":"F1345*(1-Elteq!$F$5)","v":17.47507067118099}]
["ANAMET-M",8833140,"M18 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 65",1,15.301138434574744,{"$f":"F1346*(1-Elteq!$F$5)","v":15.301138434574744}]
["ANAMET-M",8833146,"M18 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",1,16.193008070105513,{"$f":"F1347*(1-Elteq!$F$5)","v":16.193008070105513}]
["ANAMET-M",8833147,"M18 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",1,16.193008070105513,{"$f":"F1348*(1-Elteq!$F$5)","v":16.193008070105513}]
["ANAMET-M",8833160,"M12 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 65",1,16.583201035650223,{"$f":"F1349*(1-Elteq!$F$5)","v":16.583201035650223}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8833166,"M12 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",1,17.47507067118099,{"$f":"F1350*(1-Elteq!$F$5)","v":17.47507067118099}]
["ANAMET-M",8833167,"M12 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",1,19.37029364668388,{"$f":"F1351*(1-Elteq!$F$5)","v":19.37029364668388}]
["ANAMET-M",8833180,"M18 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 65",1,15.301138434574744,{"$f":"F1352*(1-Elteq!$F$5)","v":15.301138434574744}]
["ANAMET-M",8833186,"M18 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",1,16.193008070105513,{"$f":"F1353*(1-Elteq!$F$5)","v":16.193008070105513}]
["ANAMET-M",8833187,"M18 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",1,18.311198454491091,{"$f":"F1354*(1-Elteq!$F$5)","v":18.311198454491091}]
["ANAMET-M",8150060,"1/4\"","Fitting accessories for Sealtite, Ferrule, nickel plated brass",1,2.4340608803027224,{"$f":"F1355*(1-Elteq!$F$5)","v":2.4340608803027224}]
["ANAMET-M",8150100,"5/16\"","Fitting accessories for Sealtite, Ferrule, nickel plated brass",1,2.4340608803027224,{"$f":"F1356*(1-Elteq!$F$5)","v":2.4340608803027224}]
["ANAMET-M",8150110,"3/8\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,1.1055467357100148,{"$f":"F1357*(1-Elteq!$F$5)","v":1.1055467357100148}]
["ANAMET-M",8150112,"3/8\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,0.88257932682732287,{"$f":"F1358*(1-Elteq!$F$5)","v":0.88257932682732287}]
["ANAMET-M",8150113,"3/8\"","Fitting accessories for Sealtite, Ferrule, nickel plated brass",1,2.7685119936267601,{"$f":"F1359*(1-Elteq!$F$5)","v":2.7685119936267601}]
["ANAMET-M",8150117,"3/8\"","Fitting accessories for Sealtite, Ferrule, plastic (POM)",1,2.0717388408683477,{"$f":"F1360*(1-Elteq!$F$5)","v":2.0717388408683477}]
["ANAMET-M",8150160,"1/2\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,1.1705788966341335,{"$f":"F1361*(1-Elteq!$F$5)","v":1.1705788966341335}]
["ANAMET-M",8150162,"1/2\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,0.93832117904799595,{"$f":"F1362*(1-Elteq!$F$5)","v":0.93832117904799595}]
["ANAMET-M",8150163,"1/2\"","Fitting accessories for Sealtite, Ferrule, nickel plated brass",1,3.3352208245369357,{"$f":"F1363*(1-Elteq!$F$5)","v":3.3352208245369357}]
["ANAMET-M",8150167,"1/2\"","Fitting accessories for Sealtite, Ferrule, plastic (POM)",1,2.4990930412268404,{"$f":"F1364*(1-Elteq!$F$5)","v":2.4990930412268404}]
["ANAMET-M",8150210,"3/4\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,1.2449013662616977,{"$f":"F1365*(1-Elteq!$F$5)","v":1.2449013662616977}]
["ANAMET-M",8150212,"3/4\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,1.0033533399721144,{"$f":"F1366*(1-Elteq!$F$5)","v":1.0033533399721144}]
["ANAMET-M",8150213,"3/4\"","Fitting accessories for Sealtite, Ferrule, nickel plated brass",1,3.9669618163712301,{"$f":"F1367*(1-Elteq!$F$5)","v":3.9669618163712301}]
["ANAMET-M",8150217,"3/4\"","Fitting accessories for Sealtite, Ferrule, plastic (POM)",1,2.9728987851025614,{"$f":"F1368*(1-Elteq!$F$5)","v":2.9728987851025614}]
["ANAMET-M",8150290,"1\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,1.3378044532961524,{"$f":"F1369*(1-Elteq!$F$5)","v":1.3378044532961524}]
["ANAMET-M",8150292,"1\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,1.0683855008962329,{"$f":"F1370*(1-Elteq!$F$5)","v":1.0683855008962329}]
["ANAMET-M",8150293,"1\"","Fitting accessories for Sealtite, Ferrule, nickel plated brass",1,5.3140565783708276,{"$f":"F1371*(1-Elteq!$F$5)","v":5.3140565783708276}]
["ANAMET-M",8150297,"1\"","Fitting accessories for Sealtite, Ferrule, plastic (POM)",1,3.9948327424815671,{"$f":"F1372*(1-Elteq!$F$5)","v":3.9948327424815671}]
["ANAMET-M",8150362,"1.1/4\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,1.6165137143995176,{"$f":"F1373*(1-Elteq!$F$5)","v":1.6165137143995176}]
["ANAMET-M",8150363,"1 1/4\"","Fitting accessories for Sealtite, Ferrule, nickel plated brass",1,6.9770218362875731,{"$f":"F1374*(1-Elteq!$F$5)","v":6.9770218362875731}]
["ANAMET-M",8150367,"1 1/4\"","Fitting accessories for Sealtite, Ferrule, plastic (POM)",1,5.2397341087432645,{"$f":"F1375*(1-Elteq!$F$5)","v":5.2397341087432645}]
["ANAMET-M",8150422,"1 1/2\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,2.1553516191993567,{"$f":"F1376*(1-Elteq!$F$5)","v":2.1553516191993567}]
["ANAMET-M",8150423,"1 1/2\"","Fitting accessories for Sealtite, Ferrule, nickel plated brass",1,9.6247598167695418,{"$f":"F1377*(1-Elteq!$F$5)","v":9.6247598167695418}]
["ANAMET-M",8150482,"2\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,3.3816723680541636,{"$f":"F1378*(1-Elteq!$F$5)","v":3.3816723680541636}]
["ANAMET-M",8150483,"2\"","Fitting accessories for Sealtite, Ferrule, nickel plated brass",1,14.455720342561206,{"$f":"F1379*(1-Elteq!$F$5)","v":14.455720342561206}]
["ANAMET-M",8154160,"M 16","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.40877358295160221,{"$f":"F1380*(1-Elteq!$F$5)","v":0.40877358295160221}]
["ANAMET-M",8832080,"M8 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 65",1,16.295201465843416,{"$f":"F1381*(1-Elteq!$F$5)","v":16.295201465843416}]
["ANAMET-M",8832120,"M12 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 65",1,16.295201465843416,{"$f":"F1382*(1-Elteq!$F$5)","v":16.295201465843416}]
["ANAMET-M",8832180,"M18 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 65",1,18.422682158932432,{"$f":"F1383*(1-Elteq!$F$5)","v":18.422682158932432}]
["ANAMET-M",8832300,"M30 x 1,5","Special fittings for Sealtite, Proximity switch adapter, IP 65",1,26.663185978888599,{"$f":"F1384*(1-Elteq!$F$5)","v":26.663185978888599}]
["ANAMET-M",8833200,"I.D. 20 mm","Special fittings for Sealtite, Proximity switch adapter, IP 65",1,28.047441975701975,{"$f":"F1385*(1-Elteq!$F$5)","v":28.047441975701975}]
["ANAMET-M",8833340,"I.D. 34 mm","Special fittings for Sealtite, Proximity switch adapter, IP 65",1,38.359684636526488,{"$f":"F1386*(1-Elteq!$F$5)","v":38.359684636526488}]
["ANAMET-M",8840080,"M8 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 67",1,17.279974188408641,{"$f":"F1387*(1-Elteq!$F$5)","v":17.279974188408641}]
["ANAMET-M",8840120,"M12 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 67",1,17.279974188408641,{"$f":"F1388*(1-Elteq!$F$5)","v":17.279974188408641}]
["ANAMET-M",8840140,"M14 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 67",1,17.279974188408641,{"$f":"F1389*(1-Elteq!$F$5)","v":17.279974188408641}]
["ANAMET-M",8840180,"M18 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 67",1,17.279974188408641,{"$f":"F1390*(1-Elteq!$F$5)","v":17.279974188408641}]
["ANAMET-M",8840300,"M30 x 1,5","Special fittings for Sealtite, Proximity switch adapter, IP 67",1,24.247705715992769,{"$f":"F1391*(1-Elteq!$F$5)","v":24.247705715992769}]
["ANAMET-M",8154200,"M 20","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.44593481776538418,{"$f":"F1392*(1-Elteq!$F$5)","v":0.44593481776538418}]
["ANAMET-M",8154250,"M 25","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.46451543517227523,{"$f":"F1393*(1-Elteq!$F$5)","v":0.46451543517227523}]
["ANAMET-M",8154320,"M 32","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.48309605257916621,{"$f":"F1394*(1-Elteq!$F$5)","v":0.48309605257916621}]
["ANAMET-M",8154400,"M 40","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.72464407886874938,{"$f":"F1395*(1-Elteq!$F$5)","v":0.72464407886874938}]
["ANAMET-M",8154500,"M 50","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,1.1148370444134605,{"$f":"F1396*(1-Elteq!$F$5)","v":1.1148370444134605}]
["ANAMET-M",8154630,"M 63","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,1.6165137143995176,{"$f":"F1397*(1-Elteq!$F$5)","v":1.6165137143995176}]
["ANAMET-M",8155070,"PG 7 / - / -","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.39948327424815672,{"$f":"F1398*(1-Elteq!$F$5)","v":0.39948327424815672}]
["ANAMET-M",8155090,"PG 9 / M16/ -","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.39948327424815672,{"$f":"F1399*(1-Elteq!$F$5)","v":0.39948327424815672}]
["ANAMET-M",8155110,"PG 11 / - / -","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.40877358295160221,{"$f":"F1400*(1-Elteq!$F$5)","v":0.40877358295160221}]
["ANAMET-M",8155130,"PG 13,5 / - / -","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.43664450906193863,{"$f":"F1401*(1-Elteq!$F$5)","v":0.43664450906193863}]
["ANAMET-M",8155160,"PG 16 / - / 1/2\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.44593481776538418,{"$f":"F1402*(1-Elteq!$F$5)","v":0.44593481776538418}]
["ANAMET-M",8155210,"PG 21 /  - / 3/4\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.46451543517227523,{"$f":"F1403*(1-Elteq!$F$5)","v":0.46451543517227523}]
["ANAMET-M",8155290,"PG 29 / - / 1\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.48309605257916621,{"$f":"F1404*(1-Elteq!$F$5)","v":0.48309605257916621}]
["ANAMET-M",8155360,"PG 36 / - / 1 1/4\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,0.72464407886874938,{"$f":"F1405*(1-Elteq!$F$5)","v":0.72464407886874938}]
["ANAMET-M",8155420,"PG 42 / - / 1 1/2\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,1.1148370444134605,{"$f":"F1406*(1-Elteq!$F$5)","v":1.1148370444134605}]
["ANAMET-M",8155480,"PG 48 / - / 2\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",1,1.6165137143995176,{"$f":"F1407*(1-Elteq!$F$5)","v":1.6165137143995176}]
["ANAMET-M",8156160,"NPT 1/2\"","Fitting accessories for Sealtite, Seal ring round, NBR",1,6.5032160924118537E-2,{"$f":"F1408*(1-Elteq!$F$5)","v":6.5032160924118537E-2}]
["ANAMET-M",8156200,"NPT 3/4\"","Fitting accessories for Sealtite, Seal ring round, NBR",1,9.2903087034455045E-2,{"$f":"F1409*(1-Elteq!$F$5)","v":9.2903087034455045E-2}]
["ANAMET-M",8156260,"NPT 1\"","Fitting accessories for Sealtite, Seal ring round, NBR",1,0.10219339573790055,{"$f":"F1410*(1-Elteq!$F$5)","v":0.10219339573790055}]
["ANAMET-M",8156350,"NPT 1.1/4\"","Fitting accessories for Sealtite, Seal ring round, NBR",1,0.13006432184823707,{"$f":"F1411*(1-Elteq!$F$5)","v":0.13006432184823707}]
["ANAMET-M",8156400,"NPT 1.1/2\"","Fitting accessories for Sealtite, Seal ring round, NBR",1,0.15793524795857358,{"$f":"F1412*(1-Elteq!$F$5)","v":0.15793524795857358}]
["ANAMET-M",8156500,"NPT 2\"","Fitting accessories for Sealtite, Seal ring round, NBR",1,0.18580617406891009,{"$f":"F1413*(1-Elteq!$F$5)","v":0.18580617406891009}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8800070," PG 7","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,0.18580617406891009,{"$f":"F1414*(1-Elteq!$F$5)","v":0.18580617406891009}]
["ANAMET-M",8800090,"PG 9","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,0.18580617406891009,{"$f":"F1415*(1-Elteq!$F$5)","v":0.18580617406891009}]
["ANAMET-M",8800110,"PG 11","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,0.2136771001792466,{"$f":"F1416*(1-Elteq!$F$5)","v":0.2136771001792466}]
["ANAMET-M",8800130,"PG 13,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,0.2136771001792466,{"$f":"F1417*(1-Elteq!$F$5)","v":0.2136771001792466}]
["ANAMET-M",8800160,"PG 16","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,0.26941895239991959,{"$f":"F1418*(1-Elteq!$F$5)","v":0.26941895239991959}]
["ANAMET-M",8800210,"PG 21","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,0.40877358295160221,{"$f":"F1419*(1-Elteq!$F$5)","v":0.40877358295160221}]
["ANAMET-M",8800290,"PG 29","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,0.65032160924118521,{"$f":"F1420*(1-Elteq!$F$5)","v":0.65032160924118521}]
["ANAMET-M",8800360,"PG 36","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,1.5607718621788444,{"$f":"F1421*(1-Elteq!$F$5)","v":1.5607718621788444}]
["ANAMET-M",8800420,"PG 42","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,2.4712221151165039,{"$f":"F1422*(1-Elteq!$F$5)","v":2.4712221151165039}]
["ANAMET-M",8800480,"PG 48","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,2.5176736586337318,{"$f":"F1423*(1-Elteq!$F$5)","v":2.5176736586337318}]
["ANAMET-M",8801120,"M12x1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,0.18580617406891009,{"$f":"F1424*(1-Elteq!$F$5)","v":0.18580617406891009}]
["ANAMET-M",8801160,"M16 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,0.24154802628958311,{"$f":"F1425*(1-Elteq!$F$5)","v":0.24154802628958311}]
["ANAMET-M",8801200,"M20 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,0.3344511133240381,{"$f":"F1426*(1-Elteq!$F$5)","v":0.3344511133240381}]
["ANAMET-M",8801250,"M25 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,0.48309605257916621,{"$f":"F1427*(1-Elteq!$F$5)","v":0.48309605257916621}]
["ANAMET-M",8801320,"M32 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,0.60387006572395774,{"$f":"F1428*(1-Elteq!$F$5)","v":0.60387006572395774}]
["ANAMET-M",8801400,"M40 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,1.4957397012547262,{"$f":"F1429*(1-Elteq!$F$5)","v":1.4957397012547262}]
["ANAMET-M",8801500,"M50 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,2.4061899541923855,{"$f":"F1430*(1-Elteq!$F$5)","v":2.4061899541923855}]
["ANAMET-M",8801630,"M63 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,3.3909626767576091,{"$f":"F1431*(1-Elteq!$F$5)","v":3.3909626767576091}]
["ANAMET-M",8802160,"NPT 1/2\"","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,0.62245068313084884,{"$f":"F1432*(1-Elteq!$F$5)","v":0.62245068313084884}]
["ANAMET-M",8802200,"NPT 3/4\"","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,0.78967623979286783,{"$f":"F1433*(1-Elteq!$F$5)","v":0.78967623979286783}]
["ANAMET-M",8802260,"NPT 1 \"","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,1.3470947619995981,{"$f":"F1434*(1-Elteq!$F$5)","v":1.3470947619995981}]
["ANAMET-M",8802350,"NPT 1 1/4\"","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,1.9602551364270013,{"$f":"F1435*(1-Elteq!$F$5)","v":1.9602551364270013}]
["ANAMET-M",8802400,"NPT 1 1/2\"","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,3.455994837681728,{"$f":"F1436*(1-Elteq!$F$5)","v":3.455994837681728}]
["ANAMET-M",8802500,"NPT 2\"","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,6.7261835012945452,{"$f":"F1437*(1-Elteq!$F$5)","v":6.7261835012945452}]
["ANAMET-M",8803160,"NPT 1/2\"","Fitting accessories for Sealtite, Locknut, galvanised steel",1,0.34374142202748365,{"$f":"F1438*(1-Elteq!$F$5)","v":0.34374142202748365}]
["ANAMET-M",8803200,"NPT 3/4\"","Fitting accessories for Sealtite, Locknut, galvanised steel",1,0.57599913961362126,{"$f":"F1439*(1-Elteq!$F$5)","v":0.57599913961362126}]
["ANAMET-M",8803260,"NPT 1 \"","Fitting accessories for Sealtite, Locknut, galvanised steel",1,0.68748284405496729,{"$f":"F1440*(1-Elteq!$F$5)","v":0.68748284405496729}]
["ANAMET-M",8803350,"NPT 1 1/4\"","Fitting accessories for Sealtite, Locknut, galvanised steel",1,1.2170304401513612,{"$f":"F1441*(1-Elteq!$F$5)","v":1.2170304401513612}]
["ANAMET-M",8803400,"NPT 1 1/2\"","Fitting accessories for Sealtite, Locknut, galvanised steel",1,1.5236106273650625,{"$f":"F1442*(1-Elteq!$F$5)","v":1.5236106273650625}]
["ANAMET-M",8803500,"NPT 2\"","Fitting accessories for Sealtite, Locknut, galvanised steel",1,2.2110934714200297,{"$f":"F1443*(1-Elteq!$F$5)","v":2.2110934714200297}]
["ANAMET-M",8810070,"PG 9","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",1,0.74322469627564036,{"$f":"F1444*(1-Elteq!$F$5)","v":0.74322469627564036}]
["ANAMET-M",8810080,"PG 11","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",1,0.8361277833100953,{"$f":"F1445*(1-Elteq!$F$5)","v":0.8361277833100953}]
["ANAMET-M",8810090,"PG 11","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",1,0.8361277833100953,{"$f":"F1446*(1-Elteq!$F$5)","v":0.8361277833100953}]
["ANAMET-M",8810110,"PG 13,5","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",1,0.8454180920135409,{"$f":"F1447*(1-Elteq!$F$5)","v":0.8454180920135409}]
["ANAMET-M",8810120,"PG 16","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",1,1.1705788966341335,{"$f":"F1448*(1-Elteq!$F$5)","v":1.1705788966341335}]
["ANAMET-M",8810130,"PG 16","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",1,0.92903087034455045,{"$f":"F1449*(1-Elteq!$F$5)","v":0.92903087034455045}]
["ANAMET-M",8810150,"PG 21","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",1,2.2389643975303666,{"$f":"F1450*(1-Elteq!$F$5)","v":2.2389643975303666}]
["ANAMET-M",8810160,"PG 21","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",1,2.0252872973511198,{"$f":"F1451*(1-Elteq!$F$5)","v":2.0252872973511198}]
["ANAMET-M",8810210,"PG 29","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",1,3.5674785421230735,{"$f":"F1452*(1-Elteq!$F$5)","v":3.5674785421230735}]
["ANAMET-M",8810290,"PG 36","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",1,7.2464407886874929,{"$f":"F1453*(1-Elteq!$F$5)","v":7.2464407886874929}]
["ANAMET-M",8810360,"PG 42","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",1,14.390688181637087,{"$f":"F1454*(1-Elteq!$F$5)","v":14.390688181637087}]
["ANAMET-M",8810420,"PG 48","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",1,18.088231045608396,{"$f":"F1455*(1-Elteq!$F$5)","v":18.088231045608396}]
["ANAMET-M",8811070,"M 12 x 1,5","Fitting accessories for Sealtite, Adapter ISO/PG nickel plated brass",1,2.1739322366062481,{"$f":"F1456*(1-Elteq!$F$5)","v":2.1739322366062481}]
["ANAMET-M",8811090,"M 16 X 1,5","Fitting accessories for Sealtite, Adapter ISO/PG nickel plated brass",1,2.5176736586337318,{"$f":"F1457*(1-Elteq!$F$5)","v":2.5176736586337318}]
["ANAMET-M",8811110,"M 20 X 1,5","Fitting accessories for Sealtite, Adapter ISO/PG nickel plated brass",1,3.2144468113921443,{"$f":"F1458*(1-Elteq!$F$5)","v":3.2144468113921443}]
["ANAMET-M",8811160,"M 25 X 1,5","Fitting accessories for Sealtite, Adapter ISO/PG nickel plated brass",1,5.2211534913363735,{"$f":"F1459*(1-Elteq!$F$5)","v":5.2211534913363735}]
["ANAMET-M",8811210,"M 32 X 1,5","Fitting accessories for Sealtite, Adapter ISO/PG nickel plated brass",1,8.8257932682732285,{"$f":"F1460*(1-Elteq!$F$5)","v":8.8257932682732285}]
["ANAMET-M",8811290,"M 40 X 1,5","Fitting accessories for Sealtite, Adapter ISO/PG nickel plated brass",1,11.473531248755197,{"$f":"F1461*(1-Elteq!$F$5)","v":11.473531248755197}]
["ANAMET-M",8811360,"M50 x 1,5","Fitting accessories for Sealtite, Adapter ISO/PG nickel plated brass",1,15.198945038836843,{"$f":"F1462*(1-Elteq!$F$5)","v":15.198945038836843}]
["ANAMET-M",8812160,"M 12 X 1,5","Fitting accessories for Sealtite, Enlarger ISO/ISO nickel plated brass",1,1.6908361840270818,{"$f":"F1463*(1-Elteq!$F$5)","v":1.6908361840270818}]
["ANAMET-M",8812200,"M 16 X 1,5","Fitting accessories for Sealtite, Enlarger ISO/ISO nickel plated brass",1,1.7279974188408638,{"$f":"F1464*(1-Elteq!$F$5)","v":1.7279974188408638}]
["ANAMET-M",8812250,"M 20 X 1,5","Fitting accessories for Sealtite, Enlarger ISO/ISO nickel plated brass",1,2.9450278589922245,{"$f":"F1465*(1-Elteq!$F$5)","v":2.9450278589922245}]
["ANAMET-M",8812320,"M 25 X 1,5","Fitting accessories for Sealtite, Enlarger ISO/ISO nickel plated brass",1,4.5801221907986331,{"$f":"F1466*(1-Elteq!$F$5)","v":4.5801221907986331}]
["ANAMET-M",8812400,"M 32 X 1,5","Fitting accessories for Sealtite, Enlarger ISO/ISO nickel plated brass",1,6.0201200398326877,{"$f":"F1467*(1-Elteq!$F$5)","v":6.0201200398326877}]
["ANAMET-M",8812500,"M 40 X 1,5","Fitting accessories for Sealtite, Enlarger ISO/ISO nickel plated brass",1,11.780111435968898,{"$f":"F1468*(1-Elteq!$F$5)","v":11.780111435968898}]
["ANAMET-M",8812630,"M 50 X 1,5","Fitting accessories for Sealtite, Enlarger ISO/ISO nickel plated brass",1,15.905008500298706,{"$f":"F1469*(1-Elteq!$F$5)","v":15.905008500298706}]
["ANAMET-M",8820090,"PG 7","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",1,1.1334176618203515,{"$f":"F1470*(1-Elteq!$F$5)","v":1.1334176618203515}]
["ANAMET-M",8820110,"PG 9","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",1,1.1334176618203515,{"$f":"F1471*(1-Elteq!$F$5)","v":1.1334176618203515}]
["ANAMET-M",8820120,"PG 9","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",1,1.7279974188408638,{"$f":"F1472*(1-Elteq!$F$5)","v":1.7279974188408638}]
["ANAMET-M",8820130,"PG 11","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",1,1.161288587930688,{"$f":"F1473*(1-Elteq!$F$5)","v":1.161288587930688}]
["ANAMET-M",8820160,"PG 11","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",1,1.3192238358892616,{"$f":"F1474*(1-Elteq!$F$5)","v":1.3192238358892616}]
["ANAMET-M",8820170,"PG 13,5","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",1,2.39689964548894,{"$f":"F1475*(1-Elteq!$F$5)","v":2.39689964548894}]
["ANAMET-M",8820180,"PG 13,5","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",1,3.047221254730125,{"$f":"F1476*(1-Elteq!$F$5)","v":3.047221254730125}]
["ANAMET-M",8820210,"PG 16","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",1,2.39689964548894,{"$f":"F1477*(1-Elteq!$F$5)","v":2.39689964548894}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8820290,"PG 21","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",1,4.0505745947022396,{"$f":"F1478*(1-Elteq!$F$5)","v":4.0505745947022396}]
["ANAMET-M",8820360,"PG 29","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",1,8.3055359808802809,{"$f":"F1479*(1-Elteq!$F$5)","v":8.3055359808802809}]
["ANAMET-M",8820420,"PG 36","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",1,14.19559169886473,{"$f":"F1480*(1-Elteq!$F$5)","v":14.19559169886473}]
["ANAMET-M",8820480,"PG 42","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",1,15.533396152160881,{"$f":"F1481*(1-Elteq!$F$5)","v":15.533396152160881}]
["ANAMET-M",8821110,"PG 11","Fitting accessories for Sealtite, Adapter PG/ISO nickel plated brass",1,2.907866624178443,{"$f":"F1482*(1-Elteq!$F$5)","v":2.907866624178443}]
["ANAMET-M",8821160,"PG 16","Fitting accessories for Sealtite, Adapter PG/ISO nickel plated brass",1,5.5741852220673023,{"$f":"F1483*(1-Elteq!$F$5)","v":5.5741852220673023}]
["ANAMET-M",8821210,"PG 21","Fitting accessories for Sealtite, Adapter PG/ISO nickel plated brass",1,23.439448858793007,{"$f":"F1484*(1-Elteq!$F$5)","v":23.439448858793007}]
["ANAMET-M",8821290,"PG 29","Fitting accessories for Sealtite, Adapter PG/ISO nickel plated brass",1,20.652356247759354,{"$f":"F1485*(1-Elteq!$F$5)","v":20.652356247759354}]
["ANAMET-M",8821360,"PG 36","Fitting accessories for Sealtite, Adapter PG/ISO nickel plated brass",1,17.019845544712162,{"$f":"F1486*(1-Elteq!$F$5)","v":17.019845544712162}]
["ANAMET-M",8821480,"PG 48","Fitting accessories for Sealtite, Adapter PG/ISO nickel plated brass",1,25.018801338378744,{"$f":"F1487*(1-Elteq!$F$5)","v":25.018801338378744}]
["ANAMET-M",8822120,"M 16 X 1,5","Fitting accessories for Sealtite, Reducer ISO/ISO nickel plated brass",1,1.161288587930688,{"$f":"F1488*(1-Elteq!$F$5)","v":1.161288587930688}]
["ANAMET-M",8822160,"M 20 X 1,5","Fitting accessories for Sealtite, Reducer ISO/ISO nickel plated brass",1,1.3842559968133801,{"$f":"F1489*(1-Elteq!$F$5)","v":1.3842559968133801}]
["ANAMET-M",8822200,"M 25 X 1,5","Fitting accessories for Sealtite, Reducer ISO/ISO nickel plated brass",1,2.0067066799442288,{"$f":"F1490*(1-Elteq!$F$5)","v":2.0067066799442288}]
["ANAMET-M",8822250,"M 32 X 1,5","Fitting accessories for Sealtite, Reducer ISO/ISO nickel plated brass",1,3.1958661939852537,{"$f":"F1491*(1-Elteq!$F$5)","v":3.1958661939852537}]
["ANAMET-M",8822320,"M 40 X 1,5","Fitting accessories for Sealtite, Reducer ISO/ISO nickel plated brass",1,4.738057438757207,{"$f":"F1492*(1-Elteq!$F$5)","v":4.738057438757207}]
["ANAMET-M",8822400,"M 50 X 1,5","Fitting accessories for Sealtite, Reducer ISO/ISO nickel plated brass",1,10.423726365265857,{"$f":"F1493*(1-Elteq!$F$5)","v":10.423726365265857}]
["ANAMET-M",8822500,"M 63 X 1,5","Fitting accessories for Sealtite, Reducer ISO/ISO nickel plated brass",1,16.35094331806409,{"$f":"F1494*(1-Elteq!$F$5)","v":16.35094331806409}]
["ANAMET-M",8823090,"NPT 1/2\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",1,7.4694081975701847,{"$f":"F1495*(1-Elteq!$F$5)","v":7.4694081975701847}]
["ANAMET-M",8823110,"NPT 1/2\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",1,8.0732782632941422,{"$f":"F1496*(1-Elteq!$F$5)","v":8.0732782632941422}]
["ANAMET-M",8823130,"NPT 1/2\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",1,8.8629545030870105,{"$f":"F1497*(1-Elteq!$F$5)","v":8.8629545030870105}]
["ANAMET-M",8823160,"NPT 1/2\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",1,7.9153430153355693,{"$f":"F1498*(1-Elteq!$F$5)","v":7.9153430153355693}]
["ANAMET-M",8823210,"NPT 3/4\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",1,12.43972335391353,{"$f":"F1499*(1-Elteq!$F$5)","v":12.43972335391353}]
["ANAMET-M",8823260,"NPT 1\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",1,20.921775200159274,{"$f":"F1500*(1-Elteq!$F$5)","v":20.921775200159274}]
["ANAMET-M",8823290,"NPT 1\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",1,21.795064218283152,{"$f":"F1501*(1-Elteq!$F$5)","v":21.795064218283152}]
["ANAMET-M",8823300,"NPT 1 1/4\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",1,21.795064218283152,{"$f":"F1502*(1-Elteq!$F$5)","v":21.795064218283152}]
["ANAMET-M",8823360,"NPT 1 1/4\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",1,21.795064218283152,{"$f":"F1503*(1-Elteq!$F$5)","v":21.795064218283152}]
["ANAMET-M",8823400,"NPT 1 1/2\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",1,27.499313762198693,{"$f":"F1504*(1-Elteq!$F$5)","v":27.499313762198693}]
["ANAMET-M",8823420,"NPT 1 1/2\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",1,66.24919136426989,{"$f":"F1505*(1-Elteq!$F$5)","v":66.24919136426989}]
["ANAMET-M",8823480,"NPT 2\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",1,66.24919136426989,{"$f":"F1506*(1-Elteq!$F$5)","v":66.24919136426989}]
["ANAMET-M",8824100,"PG 9","Fitting accessories for Sealtite, Adapter PG/NPT nickel plated brass",1,8.0732782632941422,{"$f":"F1507*(1-Elteq!$F$5)","v":8.0732782632941422}]
["ANAMET-M",8824110,"PG 11","Fitting accessories for Sealtite, Adapter PG/NPT nickel plated brass",1,10.498048834893421,{"$f":"F1508*(1-Elteq!$F$5)","v":10.498048834893421}]
["ANAMET-M",8824120,"PG 11","Fitting accessories for Sealtite, Adapter PG/NPT nickel plated brass",1,9.9034690778729075,{"$f":"F1509*(1-Elteq!$F$5)","v":9.9034690778729075}]
["ANAMET-M",8824130,"PG 13,5","Fitting accessories for Sealtite, Adapter PG/NPT nickel plated brass",1,9.7176629038039977,{"$f":"F1510*(1-Elteq!$F$5)","v":9.7176629038039977}]
["ANAMET-M",8824160,"PG 16","Fitting accessories for Sealtite, Adapter PG/NPT nickel plated brass",1,9.7176629038039977,{"$f":"F1511*(1-Elteq!$F$5)","v":9.7176629038039977}]
["ANAMET-M",8824200,"PG 21","Fitting accessories for Sealtite, Adapter PG/NPT nickel plated brass",1,15.923589117705594,{"$f":"F1512*(1-Elteq!$F$5)","v":15.923589117705594}]
["ANAMET-M",8824350,"PG 29","Fitting accessories for Sealtite, Adapter PG/NPT nickel plated brass",1,23.541642254530906,{"$f":"F1513*(1-Elteq!$F$5)","v":23.541642254530906}]
["ANAMET-M",8824400,"PG 36","Fitting accessories for Sealtite, Adapter PG/NPT nickel plated brass",1,31.921500705038753,{"$f":"F1514*(1-Elteq!$F$5)","v":31.921500705038753}]
["ANAMET-M",8824500,"PG 48","Fitting accessories for Sealtite, Adapter PG/NPT nickel plated brass",1,81.764006899023883,{"$f":"F1515*(1-Elteq!$F$5)","v":81.764006899023883}]
["ANAMET-M",8825160,"NPT 1/2\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",1,13.991204907388928,{"$f":"F1516*(1-Elteq!$F$5)","v":13.991204907388928}]
["ANAMET-M",8825200,"NPT 1/2\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",1,3.8833490380402202,{"$f":"F1517*(1-Elteq!$F$5)","v":3.8833490380402202}]
["ANAMET-M",8825220,"NPT 1/2\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",1,7.3114729496116118,{"$f":"F1518*(1-Elteq!$F$5)","v":7.3114729496116118}]
["ANAMET-M",8825240,"NPT 3/4\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",1,8.8165029595697835,{"$f":"F1519*(1-Elteq!$F$5)","v":8.8165029595697835}]
["ANAMET-M",8825250,"NPT 3/4\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",1,8.7700514160525547,{"$f":"F1520*(1-Elteq!$F$5)","v":8.7700514160525547}]
["ANAMET-M",8825270,"NPT 3/4\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",1,10.256500808603835,{"$f":"F1521*(1-Elteq!$F$5)","v":10.256500808603835}]
["ANAMET-M",8825280,"NPT 1\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",1,14.44643003385776,{"$f":"F1522*(1-Elteq!$F$5)","v":14.44643003385776}]
["ANAMET-M",8825320,"NPT 1\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",1,29.041505006970645,{"$f":"F1523*(1-Elteq!$F$5)","v":29.041505006970645}]
["ANAMET-M",8825360,"NPT 1 1/4\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",1,50.037602676757487,{"$f":"F1524*(1-Elteq!$F$5)","v":50.037602676757487}]
["ANAMET-M",8825380,"NPT 1 1/4\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",1,41.063164469229129,{"$f":"F1525*(1-Elteq!$F$5)","v":41.063164469229129}]
["ANAMET-M",8825400,"NPT 1 1/4\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",1,31.103953539135549,{"$f":"F1526*(1-Elteq!$F$5)","v":31.103953539135549}]
["ANAMET-M",8826120,"M16 x 1,5","Fitting accessories for Sealtite, Adapter ISO/NPT nickel plated brass",1,6.1130231268671418,{"$f":"F1527*(1-Elteq!$F$5)","v":6.1130231268671418}]
["ANAMET-M",8826160,"M20 x 1,5","Fitting accessories for Sealtite, Adapter ISO/NPT nickel plated brass",1,5.8436041744672229,{"$f":"F1528*(1-Elteq!$F$5)","v":5.8436041744672229}]
["ANAMET-M",8826200,"M25 x 1,5","Fitting accessories for Sealtite, Adapter ISO/NPT nickel plated brass",1,7.4879888149770775,{"$f":"F1529*(1-Elteq!$F$5)","v":7.4879888149770775}]
["ANAMET-M",8826260,"M32 x 1,5","Fitting accessories for Sealtite, Adapter ISO/NPT nickel plated brass",1,9.0766316032662573,{"$f":"F1530*(1-Elteq!$F$5)","v":9.0766316032662573}]
["ANAMET-M",2668120,"3/8\"","Fitting accessories for Sealtite, Encap neoprene",1,0.54812821350328467,{"$f":"F1531*(1-Elteq!$F$5)","v":0.54812821350328467}]
["ANAMET-M",2668170,"1/2\"","Fitting accessories for Sealtite, Encap neoprene",1,0.63174099183429433,{"$f":"F1532*(1-Elteq!$F$5)","v":0.63174099183429433}]
["ANAMET-M",2668230,"3/4\"","Fitting accessories for Sealtite, Encap neoprene",1,1.0962564270065693,{"$f":"F1533*(1-Elteq!$F$5)","v":1.0962564270065693}]
["ANAMET-M",2668290,"1\"","Fitting accessories for Sealtite, Encap neoprene",1,1.4957397012547262,{"$f":"F1534*(1-Elteq!$F$5)","v":1.4957397012547262}]
["ANAMET-M",2668360,"1 1/4\"","Fitting accessories for Sealtite, Encap neoprene",1,2.1181903843855747,{"$f":"F1535*(1-Elteq!$F$5)","v":2.1181903843855747}]
["ANAMET-M",7830160,"M 16 x 1,5","Fitting accessories for Sealtite, Elbow fitting male/female",1,3.6046397769368554,{"$f":"F1536*(1-Elteq!$F$5)","v":3.6046397769368554}]
["ANAMET-M",7830200,"M 20 x 1,5","Fitting accessories for Sealtite, Elbow fitting male/female",1,4.1434776817366954,{"$f":"F1537*(1-Elteq!$F$5)","v":4.1434776817366954}]
["ANAMET-M",7830250,"M 25 x 1,5","Fitting accessories for Sealtite, Elbow fitting male/female",1,8.5377936984664178,{"$f":"F1538*(1-Elteq!$F$5)","v":8.5377936984664178}]
["ANAMET-M",7830320,"M 32 x 1,5","Fitting accessories for Sealtite, Elbow fitting male/female",1,14.334946329416413,{"$f":"F1539*(1-Elteq!$F$5)","v":14.334946329416413}]
["ANAMET-M",7840100,"-","Fitting accessories for Sealtite, Conduit connector, IP 67",1,7.3021826409081667,{"$f":"F1540*(1-Elteq!$F$5)","v":7.3021826409081667}]
["ANAMET-M",7840120,"-","Fitting accessories for Sealtite, Conduit connector, IP 67",1,6.1873455964947057,{"$f":"F1541*(1-Elteq!$F$5)","v":6.1873455964947057}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},7840160,"-","Fitting accessories for Sealtite, Conduit connector, IP 67",1,7.5251500497908586,{"$f":"F1542*(1-Elteq!$F$5)","v":7.5251500497908586}]
["ANAMET-M",7840200,"-","Fitting accessories for Sealtite, Conduit connector, IP 67",1,11.315596000796624,{"$f":"F1543*(1-Elteq!$F$5)","v":11.315596000796624}]
["ANAMET-M",7840260,"-","Fitting accessories for Sealtite, Conduit connector, IP 67",1,20.299324517028428,{"$f":"F1544*(1-Elteq!$F$5)","v":20.299324517028428}]
["ANAMET-M",7840350,"-","Fitting accessories for Sealtite, Conduit connector, IP 67",1,27.229894809798772,{"$f":"F1545*(1-Elteq!$F$5)","v":27.229894809798772}]
["ANAMET-M",7840400,"-","Fitting accessories for Sealtite, Conduit connector, IP 67",1,37.904459510057656,{"$f":"F1546*(1-Elteq!$F$5)","v":37.904459510057656}]
["ANAMET-M",7840500,"-","Fitting accessories for Sealtite, Conduit connector, IP 67",1,53.846629245170142,{"$f":"F1547*(1-Elteq!$F$5)","v":53.846629245170142}]
["ANAMET-M",8852160,"M 16 x 1,5","Fitting accessories for Sealtite, Swivel adapter, IP 54",1,6.6704416490738714,{"$f":"F1548*(1-Elteq!$F$5)","v":6.6704416490738714}]
["ANAMET-M",8852161,"M 16 x 1,5","Fitting accessories for Sealtite, Swivel adapter, IP 67",1,13.731076263692454,{"$f":"F1549*(1-Elteq!$F$5)","v":13.731076263692454}]
["ANAMET-M",8852200,"M 20 x 1,5","Fitting accessories for Sealtite, Swivel adapter, IP 54",1,8.3426972156940646,{"$f":"F1550*(1-Elteq!$F$5)","v":8.3426972156940646}]
["ANAMET-M",8852201,"M 20 x 1,5","Fitting accessories for Sealtite, Swivel adapter, IP 67",1,17.196361410077628,{"$f":"F1551*(1-Elteq!$F$5)","v":17.196361410077628}]
["ANAMET-M",8852250,"M 25 x 1,5","Fitting accessories for Sealtite, Swivel adapter, IP 54",1,9.9592109300935814,{"$f":"F1552*(1-Elteq!$F$5)","v":9.9592109300935814}]
["ANAMET-M",8852251,"M 25 x 1,5","Fitting accessories for Sealtite, Swivel adapter, IP 67",1,22.463966444931227,{"$f":"F1553*(1-Elteq!$F$5)","v":22.463966444931227}]
["ANAMET-M",8852320,"M 32 x 1,5","Fitting accessories for Sealtite, Swivel adapter, IP 54",1,18.134682589125624,{"$f":"F1554*(1-Elteq!$F$5)","v":18.134682589125624}]
["ANAMET-M",8852321,"M 32 x 1,5","Fitting accessories for Sealtite, Swivel adapter, IP 67",1,29.218020872336108,{"$f":"F1555*(1-Elteq!$F$5)","v":29.218020872336108}]
["ANAMET-M",8852400,"M 40 x 1,5","Fitting accessories for Sealtite, Swivel adapter, IP 54",1,32.924854045010868,{"$f":"F1556*(1-Elteq!$F$5)","v":32.924854045010868}]
["ANAMET-M",8852401,"M 40 x 1,5","Fitting accessories for Sealtite, Swivel adapter, IP 67",1,39.409489520015825,{"$f":"F1557*(1-Elteq!$F$5)","v":39.409489520015825}]
["ANAMET-M",8800119,"PG 11","Fitting accessories for Sealtite, Locknut, stainless steel 304",1,7.7666980760804405,{"$f":"F1558*(1-Elteq!$F$5)","v":7.7666980760804405}]
["ANAMET-M",8800139,"PG 13,5","Fitting accessories for Sealtite, Locknut, stainless steel 304",1,9.1323734554869311,{"$f":"F1559*(1-Elteq!$F$5)","v":9.1323734554869311}]
["ANAMET-M",8800169,"PG 16","Fitting accessories for Sealtite, Locknut, stainless steel 304",1,13.470947619995981,{"$f":"F1560*(1-Elteq!$F$5)","v":13.470947619995981}]
["ANAMET-M",8800219,"PG 21","Fitting accessories for Sealtite, Locknut, stainless steel 304",1,12.244626871141174,{"$f":"F1561*(1-Elteq!$F$5)","v":12.244626871141174}]
["ANAMET-M",8800299,"PG 29","Fitting accessories for Sealtite, Locknut, stainless steel 304",1,37.319170061740593,{"$f":"F1562*(1-Elteq!$F$5)","v":37.319170061740593}]
["ANAMET-M",8800369,"PG 36","Fitting accessories for Sealtite, Locknut, stainless steel 304",1,60.043265150368292,{"$f":"F1563*(1-Elteq!$F$5)","v":60.043265150368292}]
["ANAMET-M",8801169,"M16 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 304",1,17.019845544712162,{"$f":"F1564*(1-Elteq!$F$5)","v":17.019845544712162}]
["ANAMET-M",8801209,"M20 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 304",1,10.340113586934848,{"$f":"F1565*(1-Elteq!$F$5)","v":10.340113586934848}]
["ANAMET-M",8801259,"M25 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 304",1,14.892364851623144,{"$f":"F1566*(1-Elteq!$F$5)","v":14.892364851623144}]
["ANAMET-M",8801329,"M32 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 304",1,28.688473276239716,{"$f":"F1567*(1-Elteq!$F$5)","v":28.688473276239716}]
["ANAMET-M",8801409,"M40 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 304",1,38.833490380402203,{"$f":"F1568*(1-Elteq!$F$5)","v":38.833490380402203}]
["ANAMET-M",8802169,"NPT 1/2\"","Fitting accessories for Sealtite, Locknut, stainless steel 304",1,14.344236638119858,{"$f":"F1569*(1-Elteq!$F$5)","v":14.344236638119858}]
["ANAMET-M",8802209,"NPT 3/4\"","Fitting accessories for Sealtite, Locknut, stainless steel 304",1,17.057006779525945,{"$f":"F1570*(1-Elteq!$F$5)","v":17.057006779525945}]
["ANAMET-M",8802269,"NPT 1 \"","Fitting accessories for Sealtite, Locknut, stainless steel 304",1,30.481502856004703,{"$f":"F1571*(1-Elteq!$F$5)","v":30.481502856004703}]
["ANAMET-M",8802359,"NPT 1 1/4\"","Fitting accessories for Sealtite, Locknut, stainless steel 304",1,41.239680334594588,{"$f":"F1572*(1-Elteq!$F$5)","v":41.239680334594588}]
["ANAMET-M",2972120,"-","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,2.2018031627165846,{"$f":"F1573*(1-Elteq!$F$5)","v":2.2018031627165846}]
["ANAMET-M",2972160,"-","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,2.2018031627165846,{"$f":"F1574*(1-Elteq!$F$5)","v":2.2018031627165846}]
["ANAMET-M",2972200,"-","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,2.4712221151165039,{"$f":"F1575*(1-Elteq!$F$5)","v":2.4712221151165039}]
["ANAMET-M",2972260,"-","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,3.59534946823341,{"$f":"F1576*(1-Elteq!$F$5)","v":3.59534946823341}]
["ANAMET-M",2972350,"-","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,8.4263099940250736,{"$f":"F1577*(1-Elteq!$F$5)","v":8.4263099940250736}]
["ANAMET-M",2972400,"-","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,10.776758095996785,{"$f":"F1578*(1-Elteq!$F$5)","v":10.776758095996785}]
["ANAMET-M",2972500,"-","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,14.957397012547263,{"$f":"F1579*(1-Elteq!$F$5)","v":14.957397012547263}]
["ANAMET-M",2972630,"-","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,63.452808444532792,{"$f":"F1580*(1-Elteq!$F$5)","v":63.452808444532792}]
["ANAMET-M",2972750,"-","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,85.842452419836462,{"$f":"F1581*(1-Elteq!$F$5)","v":85.842452419836462}]
["ANAMET-M",2974160,"-","Fitting accessories for Sealtite, Locknut, galvanised steel",1,0.5109669786895028,{"$f":"F1582*(1-Elteq!$F$5)","v":0.5109669786895028}]
["ANAMET-M",2974200,"-","Fitting accessories for Sealtite, Locknut, galvanised steel",1,0.85470840071698639,{"$f":"F1583*(1-Elteq!$F$5)","v":0.85470840071698639}]
["ANAMET-M",2974260,"-","Fitting accessories for Sealtite, Locknut, galvanised steel",1,1.4771590838478352,{"$f":"F1584*(1-Elteq!$F$5)","v":1.4771590838478352}]
["ANAMET-M",2974350,"-","Fitting accessories for Sealtite, Locknut, galvanised steel",1,1.7837392710615367,{"$f":"F1585*(1-Elteq!$F$5)","v":1.7837392710615367}]
["ANAMET-M",2974400,"-","Fitting accessories for Sealtite, Locknut, galvanised steel",1,2.7127701414060872,{"$f":"F1586*(1-Elteq!$F$5)","v":2.7127701414060872}]
["ANAMET-M",2974500,"-","Fitting accessories for Sealtite, Locknut, galvanised steel",1,4.0784455208125756,{"$f":"F1587*(1-Elteq!$F$5)","v":4.0784455208125756}]
["ANAMET-M",2975120,"-","Fitting accessories for Sealtite, Nut with extrenal lug",1,6.921279984066901,{"$f":"F1588*(1-Elteq!$F$5)","v":6.921279984066901}]
["ANAMET-M",2975160,"-","Fitting accessories for Sealtite, Nut with extrenal lug",1,10.590951921927875,{"$f":"F1589*(1-Elteq!$F$5)","v":10.590951921927875}]
["ANAMET-M",2975200,"-","Fitting accessories for Sealtite, Nut with extrenal lug",1,19.045132842063285,{"$f":"F1590*(1-Elteq!$F$5)","v":19.045132842063285}]
["ANAMET-M",2975260,"-","Fitting accessories for Sealtite, Nut with extrenal lug",1,29.543181676956703,{"$f":"F1591*(1-Elteq!$F$5)","v":29.543181676956703}]
["ANAMET-M",2975350,"-","Fitting accessories for Sealtite, Nut with extrenal lug",1,75.344403584943038,{"$f":"F1592*(1-Elteq!$F$5)","v":75.344403584943038}]
["ANAMET-M",8150115,"3/8\"","Fitting accessories for Sealtite, Ferrule, stainless steel 304",1,3.1679952678749173,{"$f":"F1593*(1-Elteq!$F$5)","v":3.1679952678749173}]
["ANAMET-M",8150165,"1/2\"","Fitting accessories for Sealtite, Ferrule, stainless steel 304",1,3.7904459510057658,{"$f":"F1594*(1-Elteq!$F$5)","v":3.7904459510057658}]
["ANAMET-M",8150215,"3/4\"","Fitting accessories for Sealtite, Ferrule, stainless steel 304",1,4.4407675602469512,{"$f":"F1595*(1-Elteq!$F$5)","v":4.4407675602469512}]
["ANAMET-M",8150295,"1\"","Fitting accessories for Sealtite, Ferrule, stainless steel 304",1,5.0632182433777997,{"$f":"F1596*(1-Elteq!$F$5)","v":5.0632182433777997}]
["ANAMET-M",8150365,"1 1/4\"","Fitting accessories for Sealtite, Ferrule, stainless steel 304",1,5.4069596654052834,{"$f":"F1597*(1-Elteq!$F$5)","v":5.4069596654052834}]
["ANAMET-M",8150425,"1 1/2\"","Fitting accessories for Sealtite, Ferrule, stainless steel 304",1,5.6670883091017572,{"$f":"F1598*(1-Elteq!$F$5)","v":5.6670883091017572}]
["ANAMET-M",8150485,"2\"","Fitting accessories for Sealtite, Ferrule, stainless steel 304",1,7.097795849432365,{"$f":"F1599*(1-Elteq!$F$5)","v":7.097795849432365}]
["ANAMET-M",8156160,"NPT 1/2\"","Fitting accessories for Sealtite, Seal ring round, NBR",1,6.5032160924118537E-2,{"$f":"F1600*(1-Elteq!$F$5)","v":6.5032160924118537E-2}]
["ANAMET-M",8156200,"NPT 3/4\"","Fitting accessories for Sealtite, Seal ring round, NBR",1,9.2903087034455045E-2,{"$f":"F1601*(1-Elteq!$F$5)","v":9.2903087034455045E-2}]
["ANAMET-M",8156260,"NPT 1\"","Fitting accessories for Sealtite, Seal ring round, NBR",1,0.10219339573790055,{"$f":"F1602*(1-Elteq!$F$5)","v":0.10219339573790055}]
["ANAMET-M",8156350,"NPT 1.1/4\"","Fitting accessories for Sealtite, Seal ring round, NBR",1,0.13006432184823707,{"$f":"F1603*(1-Elteq!$F$5)","v":0.13006432184823707}]
["ANAMET-M",8156400,"NPT 1.1/2\"","Fitting accessories for Sealtite, Seal ring round, NBR",1,0.15793524795857358,{"$f":"F1604*(1-Elteq!$F$5)","v":0.15793524795857358}]
["ANAMET-M",8156500,"NPT 2\"","Fitting accessories for Sealtite, Seal ring round, NBR",1,0.18580617406891009,{"$f":"F1605*(1-Elteq!$F$5)","v":0.18580617406891009}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8801168,"M16 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 316",1,16.945523075084598,{"$f":"F1606*(1-Elteq!$F$5)","v":16.945523075084598}]
["ANAMET-M",8801208,"M20 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 316",1,19.509648277235559,{"$f":"F1607*(1-Elteq!$F$5)","v":19.509648277235559}]
["ANAMET-M",8801258,"M25 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 316",1,23.355836080461998,{"$f":"F1608*(1-Elteq!$F$5)","v":23.355836080461998}]
["ANAMET-M",8801328,"M32 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 316",1,41.63916360884275,{"$f":"F1609*(1-Elteq!$F$5)","v":41.63916360884275}]
["ANAMET-M",8801408,"M40 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 316",1,57.302624082851864,{"$f":"F1610*(1-Elteq!$F$5)","v":57.302624082851864}]
["ANAMET-M",8802168,"NPT 1/2\"","Fitting accessories for Sealtite, Locknut, stainless steel 316",1,20.79171087831104,{"$f":"F1611*(1-Elteq!$F$5)","v":20.79171087831104}]
["ANAMET-M",8802208,"NPT 3/4\"","Fitting accessories for Sealtite, Locknut, stainless steel 316",1,24.693640533758149,{"$f":"F1612*(1-Elteq!$F$5)","v":24.693640533758149}]
["ANAMET-M",8802268,"NPT 1\"","Fitting accessories for Sealtite, Locknut, stainless steel 316",1,44.203288810993712,{"$f":"F1613*(1-Elteq!$F$5)","v":44.203288810993712}]
["ANAMET-M",8802358,"NPT 1.1/4\"","Fitting accessories for Sealtite, Locknut, stainless steel 316",1,59.866749285002825,{"$f":"F1614*(1-Elteq!$F$5)","v":59.866749285002825}]
["ANAMET-M",8802408,"NPT 1.1/2\"","Fitting accessories for Sealtite, Locknut, stainless steel 316",1,97.548241386177793,{"$f":"F1615*(1-Elteq!$F$5)","v":97.548241386177793}]
["ANAMET-M",8803169,"NPT 1/2\"","Fitting accessories for Sealtite, Locknut, stainless steel 304",1,1.9881260625373383,{"$f":"F1616*(1-Elteq!$F$5)","v":1.9881260625373383}]
["ANAMET-M",8803209,"NPT 3/4\"","Fitting accessories for Sealtite, Locknut, stainless steel 304",1,2.8892860067715516,{"$f":"F1617*(1-Elteq!$F$5)","v":2.8892860067715516}]
["ANAMET-M",8803269,"NPT 1 \"","Fitting accessories for Sealtite, Locknut, stainless steel 304",1,5.1375407130053636,{"$f":"F1618*(1-Elteq!$F$5)","v":5.1375407130053636}]
["ANAMET-M",8803359,"NPT 1 1/4\"","Fitting accessories for Sealtite, Locknut, stainless steel 304",1,5.7228301613224302,{"$f":"F1619*(1-Elteq!$F$5)","v":5.7228301613224302}]
["ANAMET-M",8803409,"NPT 1 1/2\"","Fitting accessories for Sealtite, Locknut, stainless steel 304",1,7.4694081975701847,{"$f":"F1620*(1-Elteq!$F$5)","v":7.4694081975701847}]
["ANAMET-M",8803509,"NPT 2\"","Fitting accessories for Sealtite, Locknut, stainless steel 304",1,11.640756805417215,{"$f":"F1621*(1-Elteq!$F$5)","v":11.640756805417215}]
["ANAMET-M",2970160,"-","Fitting accessories for Sealtite, Sealing gasket, neoprene/steel",1,2.2668353236407031,{"$f":"F1622*(1-Elteq!$F$5)","v":2.2668353236407031}]
["ANAMET-M",2970200,"-","Fitting accessories for Sealtite, Sealing gasket, neoprene/steel",1,2.2668353236407031,{"$f":"F1623*(1-Elteq!$F$5)","v":2.2668353236407031}]
["ANAMET-M",2970260,"-","Fitting accessories for Sealtite, Sealing gasket, neoprene/steel",1,3.539607616012737,{"$f":"F1624*(1-Elteq!$F$5)","v":3.539607616012737}]
["ANAMET-M",2970350,"-","Fitting accessories for Sealtite, Sealing gasket, neoprene/steel",1,6.1966359051981517,{"$f":"F1625*(1-Elteq!$F$5)","v":6.1966359051981517}]
["ANAMET-M",2970400,"-","Fitting accessories for Sealtite, Sealing gasket, neoprene/steel",1,7.2836020235012748,{"$f":"F1626*(1-Elteq!$F$5)","v":7.2836020235012748}]
["ANAMET-M",2970500,"-","Fitting accessories for Sealtite, Sealing gasket, neoprene/steel",1,8.9744382075283582,{"$f":"F1627*(1-Elteq!$F$5)","v":8.9744382075283582}]
["ANAMET-M",2973120,"-","Fitting accessories for Sealtite, Wire mesh, galvanised steel",1,53.512178131846106,{"$f":"F1628*(1-Elteq!$F$5)","v":53.512178131846106}]
["ANAMET-M",2973160,"-","Fitting accessories for Sealtite, Wire mesh, galvanised steel",1,57.135398526189853,{"$f":"F1629*(1-Elteq!$F$5)","v":57.135398526189853}]
["ANAMET-M",2973200,"-","Fitting accessories for Sealtite, Wire mesh, galvanised steel",1,69.398606014737922,{"$f":"F1630*(1-Elteq!$F$5)","v":69.398606014737922}]
["ANAMET-M",2973260,"-","Fitting accessories for Sealtite, Wire mesh, galvanised steel",1,77.759883847838879,{"$f":"F1631*(1-Elteq!$F$5)","v":77.759883847838879}]
["ANAMET-M",2973350,"-","Fitting accessories for Sealtite, Wire mesh, galvanised steel",1,89.094060466042393,{"$f":"F1632*(1-Elteq!$F$5)","v":89.094060466042393}]
["ANAMET-M",2973400,"-","Fitting accessories for Sealtite, Wire mesh, galvanised steel",1,130.40806327026453,{"$f":"F1633*(1-Elteq!$F$5)","v":130.40806327026453}]
["ANAMET-M",2973500,"-","Fitting accessories for Sealtite, Wire mesh, galvanised steel",1,196.51790000398273,{"$f":"F1634*(1-Elteq!$F$5)","v":196.51790000398273}]
["ANAMET-M",8850160,"1/2\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",1,0.1765158653654646,{"$f":"F1635*(1-Elteq!$F$5)","v":0.1765158653654646}]
["ANAMET-M",8850162,"1/2\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",1,0.28799956980681063,{"$f":"F1636*(1-Elteq!$F$5)","v":0.28799956980681063}]
["ANAMET-M",8850200,"3/4\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",1,0.26012864369647415,{"$f":"F1637*(1-Elteq!$F$5)","v":0.26012864369647415}]
["ANAMET-M",8850202,"3/4\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",1,0.37161234813782018,{"$f":"F1638*(1-Elteq!$F$5)","v":0.37161234813782018}]
["ANAMET-M",8850260,"1\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",1,0.35303173073092919,{"$f":"F1639*(1-Elteq!$F$5)","v":0.35303173073092919}]
["ANAMET-M",8850262,"1\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",1,0.66890222664807619,{"$f":"F1640*(1-Elteq!$F$5)","v":0.66890222664807619}]
["ANAMET-M",8850350,"1.1/4\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",1,0.4273542003584932,{"$f":"F1641*(1-Elteq!$F$5)","v":0.4273542003584932}]
["ANAMET-M",8850352,"1.1/4\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",1,1.0683855008962329,{"$f":"F1642*(1-Elteq!$F$5)","v":1.0683855008962329}]
["ANAMET-M",8850402,"1.1/2\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",1,1.161288587930688,{"$f":"F1643*(1-Elteq!$F$5)","v":1.161288587930688}]
["ANAMET-M",8850502,"2\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",1,1.7372877275443095,{"$f":"F1644*(1-Elteq!$F$5)","v":1.7372877275443095}]
["ANAMET-M",8853060,"1/4\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",1,1.7930295797649822,{"$f":"F1645*(1-Elteq!$F$5)","v":1.7930295797649822}]
["ANAMET-M",8853100,"5/16\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",1,1.8394811232822095,{"$f":"F1646*(1-Elteq!$F$5)","v":1.8394811232822095}]
["ANAMET-M",8853120,"3/8\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",1,2.1553516191993567,{"$f":"F1647*(1-Elteq!$F$5)","v":2.1553516191993567}]
["ANAMET-M",8853160,"1/2\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",1,2.1553516191993567,{"$f":"F1648*(1-Elteq!$F$5)","v":2.1553516191993567}]
["ANAMET-M",8853200,"3/4\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",1,2.303996558454485,{"$f":"F1649*(1-Elteq!$F$5)","v":2.303996558454485}]
["ANAMET-M",8853260,"1\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",1,2.6663185978888597,{"$f":"F1650*(1-Elteq!$F$5)","v":2.6663185978888597}]
["ANAMET-M",8853350,"1.1/4\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",1,3.1215437243576889,{"$f":"F1651*(1-Elteq!$F$5)","v":3.1215437243576889}]
["ANAMET-M",8853400,"1.1/2\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",1,4.5615415733917422,{"$f":"F1652*(1-Elteq!$F$5)","v":4.5615415733917422}]
["ANAMET-M",8853500,"2\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",1,6.5961191794463083,{"$f":"F1653*(1-Elteq!$F$5)","v":6.5961191794463083}]
["ANAMET-M",8260160,"M 16 x 1,5","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",1,42.949097136028563,{"$f":"F1654*(1-Elteq!$F$5)","v":42.949097136028563}]
["ANAMET-M",8260169,"M 16 x 1,5","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",1,111.37222073690469,{"$f":"F1655*(1-Elteq!$F$5)","v":111.37222073690469}]
["ANAMET-M",8260200,"M 20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",1,43.87812800637311,{"$f":"F1656*(1-Elteq!$F$5)","v":43.87812800637311}]
["ANAMET-M",8260209,"M 20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",1,132.81425322445693,{"$f":"F1657*(1-Elteq!$F$5)","v":132.81425322445693}]
["ANAMET-M",8260250,"M 25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",1,59.197847058354753,{"$f":"F1658*(1-Elteq!$F$5)","v":59.197847058354753}]
["ANAMET-M",8260259,"M 25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",1,157.87950610635289,{"$f":"F1659*(1-Elteq!$F$5)","v":157.87950610635289}]
["ANAMET-M",8260320,"M 32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",1,107.72112941645062,{"$f":"F1660*(1-Elteq!$F$5)","v":107.72112941645062}]
["ANAMET-M",8260329,"M 32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",1,231.63526690300677,{"$f":"F1661*(1-Elteq!$F$5)","v":231.63526690300677}]
["ANAMET-M",8260400,"M 40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",1,137.35721418044176,{"$f":"F1662*(1-Elteq!$F$5)","v":137.35721418044176}]
["ANAMET-M",8260409,"M 40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",1,321.2495846564421,{"$f":"F1663*(1-Elteq!$F$5)","v":321.2495846564421}]
["ANAMET-M",8270120,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",1,42.949097136028563,{"$f":"F1664*(1-Elteq!$F$5)","v":42.949097136028563}]
["ANAMET-M",8270129,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",1,111.37222073690469,{"$f":"F1665*(1-Elteq!$F$5)","v":111.37222073690469}]
["ANAMET-M",8270160,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",1,43.87812800637311,{"$f":"F1666*(1-Elteq!$F$5)","v":43.87812800637311}]
["ANAMET-M",8270169,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",1,132.81425322445693,{"$f":"F1667*(1-Elteq!$F$5)","v":132.81425322445693}]
["ANAMET-M",8270200,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",1,59.197847058354753,{"$f":"F1668*(1-Elteq!$F$5)","v":59.197847058354753}]
["ANAMET-M",8270209,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",1,157.87950610635289,{"$f":"F1669*(1-Elteq!$F$5)","v":157.87950610635289}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8270260,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",1,107.72112941645062,{"$f":"F1670*(1-Elteq!$F$5)","v":107.72112941645062}]
["ANAMET-M",8270269,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",1,231.63526690300677,{"$f":"F1671*(1-Elteq!$F$5)","v":231.63526690300677}]
["ANAMET-M",8270350,"NPT 1.1/4\"","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",1,137.35721418044176,{"$f":"F1672*(1-Elteq!$F$5)","v":137.35721418044176}]
["ANAMET-M",8270359,"NPT 1.1/4\"","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",1,321.2495846564421,{"$f":"F1673*(1-Elteq!$F$5)","v":321.2495846564421}]
["ANAMET-M",8220080,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",1,31.512727122087153,{"$f":"F1674*(1-Elteq!$F$5)","v":31.512727122087153}]
["ANAMET-M",8220090,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",1,29.171569328818883,{"$f":"F1675*(1-Elteq!$F$5)","v":29.171569328818883}]
["ANAMET-M",8220093,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",1,31.438404652459589,{"$f":"F1676*(1-Elteq!$F$5)","v":31.438404652459589}]
["ANAMET-M",8220100,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",1,29.171569328818883,{"$f":"F1677*(1-Elteq!$F$5)","v":29.171569328818883}]
["ANAMET-M",8220103,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",1,31.438404652459589,{"$f":"F1678*(1-Elteq!$F$5)","v":31.438404652459589}]
["ANAMET-M",8220110,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 7-10 mm",1,29.171569328818883,{"$f":"F1679*(1-Elteq!$F$5)","v":29.171569328818883}]
["ANAMET-M",8220113,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 7-10 mm",1,31.438404652459589,{"$f":"F1680*(1-Elteq!$F$5)","v":31.438404652459589}]
["ANAMET-M",8220120,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 5,5-8 mm",1,33.361498554072803,{"$f":"F1681*(1-Elteq!$F$5)","v":33.361498554072803}]
["ANAMET-M",8220123,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 5,5-8 mm",1,34.97801226847232,{"$f":"F1682*(1-Elteq!$F$5)","v":34.97801226847232}]
["ANAMET-M",8220130,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 8-10,5 mm",1,33.361498554072803,{"$f":"F1683*(1-Elteq!$F$5)","v":33.361498554072803}]
["ANAMET-M",8220133,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 8-10,5 mm",1,34.97801226847232,{"$f":"F1684*(1-Elteq!$F$5)","v":34.97801226847232}]
["ANAMET-M",8220140,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",1,33.361498554072803,{"$f":"F1685*(1-Elteq!$F$5)","v":33.361498554072803}]
["ANAMET-M",8220143,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",1,34.97801226847232,{"$f":"F1686*(1-Elteq!$F$5)","v":34.97801226847232}]
["ANAMET-M",8220150,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",1,42.503162318263186,{"$f":"F1687*(1-Elteq!$F$5)","v":42.503162318263186}]
["ANAMET-M",8220153,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",1,45.271674311889939,{"$f":"F1688*(1-Elteq!$F$5)","v":45.271674311889939}]
["ANAMET-M",8220180,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 13-15,5 mm",1,42.503162318263186,{"$f":"F1689*(1-Elteq!$F$5)","v":42.503162318263186}]
["ANAMET-M",8220183,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 13-15,5 mm",1,45.271674311889939,{"$f":"F1690*(1-Elteq!$F$5)","v":45.271674311889939}]
["ANAMET-M",8220190,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15,5-18 mm",1,42.503162318263186,{"$f":"F1691*(1-Elteq!$F$5)","v":42.503162318263186}]
["ANAMET-M",8220193,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15,5-18 mm",1,45.271674311889939,{"$f":"F1692*(1-Elteq!$F$5)","v":45.271674311889939}]
["ANAMET-M",8220230,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15-18 mm",1,86.920128229436145,{"$f":"F1693*(1-Elteq!$F$5)","v":86.920128229436145}]
["ANAMET-M",8220233,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15-18 mm",1,90.914960971917708,{"$f":"F1694*(1-Elteq!$F$5)","v":90.914960971917708}]
["ANAMET-M",8220240,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 18-21 mm",1,86.920128229436145,{"$f":"F1695*(1-Elteq!$F$5)","v":86.920128229436145}]
["ANAMET-M",8220243,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 18-21 mm",1,90.914960971917708,{"$f":"F1696*(1-Elteq!$F$5)","v":90.914960971917708}]
["ANAMET-M",8220250,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-23,5 mm",1,86.920128229436145,{"$f":"F1697*(1-Elteq!$F$5)","v":86.920128229436145}]
["ANAMET-M",8220253,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-23,5 mm",1,90.914960971917708,{"$f":"F1698*(1-Elteq!$F$5)","v":90.914960971917708}]
["ANAMET-M",8220290,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-24 mm",1,127.10071337183795,{"$f":"F1699*(1-Elteq!$F$5)","v":127.10071337183795}]
["ANAMET-M",8220293,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-24 mm",1,136.42818331009724,{"$f":"F1700*(1-Elteq!$F$5)","v":136.42818331009724}]
["ANAMET-M",8220300,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 24-27 mm",1,127.10071337183795,{"$f":"F1701*(1-Elteq!$F$5)","v":127.10071337183795}]
["ANAMET-M",8220303,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 24-27 mm",1,136.42818331009724,{"$f":"F1702*(1-Elteq!$F$5)","v":136.42818331009724}]
["ANAMET-M",8220310,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 27-30 mm",1,127.10071337183795,{"$f":"F1703*(1-Elteq!$F$5)","v":127.10071337183795}]
["ANAMET-M",8220313,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 27-30 mm",1,136.42818331009724,{"$f":"F1704*(1-Elteq!$F$5)","v":136.42818331009724}]
["ANAMET-M",8240100,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",1,29.171569328818883,{"$f":"F1705*(1-Elteq!$F$5)","v":29.171569328818883}]
["ANAMET-M",8240103,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",1,31.438404652459589,{"$f":"F1706*(1-Elteq!$F$5)","v":31.438404652459589}]
["ANAMET-M",8240110,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 7-10 mm",1,29.171569328818883,{"$f":"F1707*(1-Elteq!$F$5)","v":29.171569328818883}]
["ANAMET-M",8240113,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 7-10 mm",1,31.438404652459589,{"$f":"F1708*(1-Elteq!$F$5)","v":31.438404652459589}]
["ANAMET-M",8240120,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 5,5-8 mm",1,33.361498554072803,{"$f":"F1709*(1-Elteq!$F$5)","v":33.361498554072803}]
["ANAMET-M",8240123,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 5,5-8 mm",1,34.97801226847232,{"$f":"F1710*(1-Elteq!$F$5)","v":34.97801226847232}]
["ANAMET-M",8240130,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 8-10,5 mm",1,33.361498554072803,{"$f":"F1711*(1-Elteq!$F$5)","v":33.361498554072803}]
["ANAMET-M",8240133,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 8-10,5 mm",1,34.97801226847232,{"$f":"F1712*(1-Elteq!$F$5)","v":34.97801226847232}]
["ANAMET-M",8240140,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",1,33.361498554072803,{"$f":"F1713*(1-Elteq!$F$5)","v":33.361498554072803}]
["ANAMET-M",8240143,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",1,34.97801226847232,{"$f":"F1714*(1-Elteq!$F$5)","v":34.97801226847232}]
["ANAMET-M",8240150,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",1,42.503162318263186,{"$f":"F1715*(1-Elteq!$F$5)","v":42.503162318263186}]
["ANAMET-M",8240153,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",1,45.271674311889939,{"$f":"F1716*(1-Elteq!$F$5)","v":45.271674311889939}]
["ANAMET-M",8240180,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 13-15,5 mm",1,42.503162318263186,{"$f":"F1717*(1-Elteq!$F$5)","v":42.503162318263186}]
["ANAMET-M",8240183,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 13-15,5 mm",1,45.271674311889939,{"$f":"F1718*(1-Elteq!$F$5)","v":45.271674311889939}]
["ANAMET-M",8240190,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15,5-18 mm",1,42.503162318263186,{"$f":"F1719*(1-Elteq!$F$5)","v":42.503162318263186}]
["ANAMET-M",8240193,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15,5-18 mm",1,45.271674311889939,{"$f":"F1720*(1-Elteq!$F$5)","v":45.271674311889939}]
["ANAMET-M",8240230,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15-18 mm",1,86.920128229436145,{"$f":"F1721*(1-Elteq!$F$5)","v":86.920128229436145}]
["ANAMET-M",8240233,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15-18 mm",1,90.914960971917708,{"$f":"F1722*(1-Elteq!$F$5)","v":90.914960971917708}]
["ANAMET-M",8240240,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 18-21 mm",1,86.920128229436145,{"$f":"F1723*(1-Elteq!$F$5)","v":86.920128229436145}]
["ANAMET-M",8240243,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 18-21 mm",1,90.914960971917708,{"$f":"F1724*(1-Elteq!$F$5)","v":90.914960971917708}]
["ANAMET-M",8240250,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-23,5 mm",1,86.920128229436145,{"$f":"F1725*(1-Elteq!$F$5)","v":86.920128229436145}]
["ANAMET-M",8240253,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-23,5 mm",1,90.914960971917708,{"$f":"F1726*(1-Elteq!$F$5)","v":90.914960971917708}]
["ANAMET-M",8222090,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",1,31.42911434375614,{"$f":"F1727*(1-Elteq!$F$5)","v":31.42911434375614}]
["ANAMET-M",8222093,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",1,33.686659358693397,{"$f":"F1728*(1-Elteq!$F$5)","v":33.686659358693397}]
["ANAMET-M",8222100,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",1,30.193503286197888,{"$f":"F1729*(1-Elteq!$F$5)","v":30.193503286197888}]
["ANAMET-M",8222103,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",1,32.460338609838587,{"$f":"F1730*(1-Elteq!$F$5)","v":32.460338609838587}]
["ANAMET-M",8222110,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 7-10 mm",1,30.193503286197888,{"$f":"F1731*(1-Elteq!$F$5)","v":30.193503286197888}]
["ANAMET-M",8222113,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 7-10 mm",1,32.460338609838587,{"$f":"F1732*(1-Elteq!$F$5)","v":32.460338609838587}]
["ANAMET-M",8222120,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 5,5-8 mm",1,34.597109611631055,{"$f":"F1733*(1-Elteq!$F$5)","v":34.597109611631055}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8222123,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 5,5-8 mm",1,36.20433301732713,{"$f":"F1734*(1-Elteq!$F$5)","v":36.20433301732713}]
["ANAMET-M",8222130,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 8-10,5 mm",1,34.597109611631055,{"$f":"F1735*(1-Elteq!$F$5)","v":34.597109611631055}]
["ANAMET-M",8222133,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 8-10,5 mm",1,36.20433301732713,{"$f":"F1736*(1-Elteq!$F$5)","v":36.20433301732713}]
["ANAMET-M",8222140,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",1,34.597109611631055,{"$f":"F1737*(1-Elteq!$F$5)","v":34.597109611631055}]
["ANAMET-M",8222143,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",1,36.20433301732713,{"$f":"F1738*(1-Elteq!$F$5)","v":36.20433301732713}]
["ANAMET-M",8222150,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",1,44.110385723959254,{"$f":"F1739*(1-Elteq!$F$5)","v":44.110385723959254}]
["ANAMET-M",8222153,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",1,46.888188026289463,{"$f":"F1740*(1-Elteq!$F$5)","v":46.888188026289463}]
["ANAMET-M",8222180,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 13-15,5 mm",1,44.110385723959254,{"$f":"F1741*(1-Elteq!$F$5)","v":44.110385723959254}]
["ANAMET-M",8222183,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 13-15,5 mm",1,46.888188026289463,{"$f":"F1742*(1-Elteq!$F$5)","v":46.888188026289463}]
["ANAMET-M",8222190,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15,5-18 mm",1,44.110385723959254,{"$f":"F1743*(1-Elteq!$F$5)","v":44.110385723959254}]
["ANAMET-M",8222193,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15,5-18 mm",1,46.888188026289463,{"$f":"F1744*(1-Elteq!$F$5)","v":46.888188026289463}]
["ANAMET-M",8222230,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15-18 mm",1,88.536641943835662,{"$f":"F1745*(1-Elteq!$F$5)","v":88.536641943835662}]
["ANAMET-M",8222233,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15-18 mm",1,92.53147468631721,{"$f":"F1746*(1-Elteq!$F$5)","v":92.53147468631721}]
["ANAMET-M",8222240,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 18-21 mm",1,88.536641943835662,{"$f":"F1747*(1-Elteq!$F$5)","v":88.536641943835662}]
["ANAMET-M",8222243,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 18-21 mm",1,92.53147468631721,{"$f":"F1748*(1-Elteq!$F$5)","v":92.53147468631721}]
["ANAMET-M",8222250,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-23,5 mm",1,88.536641943835662,{"$f":"F1749*(1-Elteq!$F$5)","v":88.536641943835662}]
["ANAMET-M",8222253,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-23,5 mm",1,92.53147468631721,{"$f":"F1750*(1-Elteq!$F$5)","v":92.53147468631721}]
["ANAMET-M",8222290,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-24 mm",1,130.12006370045773,{"$f":"F1751*(1-Elteq!$F$5)","v":130.12006370045773}]
["ANAMET-M",8222293,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-24 mm",1,139.47540456482736,{"$f":"F1752*(1-Elteq!$F$5)","v":139.47540456482736}]
["ANAMET-M",8222300,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 24-27 mm",1,130.12006370045773,{"$f":"F1753*(1-Elteq!$F$5)","v":130.12006370045773}]
["ANAMET-M",8222303,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 24-27 mm",1,139.47540456482736,{"$f":"F1754*(1-Elteq!$F$5)","v":139.47540456482736}]
["ANAMET-M",8222310,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 27-30 mm",1,130.12006370045773,{"$f":"F1755*(1-Elteq!$F$5)","v":130.12006370045773}]
["ANAMET-M",8222313,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 27-30 mm",1,139.47540456482736,{"$f":"F1756*(1-Elteq!$F$5)","v":139.47540456482736}]
["ANAMET-M",8242100,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",1,30.193503286197888,{"$f":"F1757*(1-Elteq!$F$5)","v":30.193503286197888}]
["ANAMET-M",8242103,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",1,32.460338609838587,{"$f":"F1758*(1-Elteq!$F$5)","v":32.460338609838587}]
["ANAMET-M",8242110,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 7-10 mm",1,30.193503286197888,{"$f":"F1759*(1-Elteq!$F$5)","v":30.193503286197888}]
["ANAMET-M",8242113,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 7-10 mm",1,32.460338609838587,{"$f":"F1760*(1-Elteq!$F$5)","v":32.460338609838587}]
["ANAMET-M",8242120,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 5,5-8 mm",1,34.597109611631055,{"$f":"F1761*(1-Elteq!$F$5)","v":34.597109611631055}]
["ANAMET-M",8242123,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 5,5-8 mm",1,36.20433301732713,{"$f":"F1762*(1-Elteq!$F$5)","v":36.20433301732713}]
["ANAMET-M",8242130,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 8-10,5 mm",1,34.597109611631055,{"$f":"F1763*(1-Elteq!$F$5)","v":34.597109611631055}]
["ANAMET-M",8242133,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 8-10,5 mm",1,36.20433301732713,{"$f":"F1764*(1-Elteq!$F$5)","v":36.20433301732713}]
["ANAMET-M",8242140,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",1,34.597109611631055,{"$f":"F1765*(1-Elteq!$F$5)","v":34.597109611631055}]
["ANAMET-M",8242143,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",1,36.20433301732713,{"$f":"F1766*(1-Elteq!$F$5)","v":36.20433301732713}]
["ANAMET-M",8242150,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",1,44.110385723959254,{"$f":"F1767*(1-Elteq!$F$5)","v":44.110385723959254}]
["ANAMET-M",8242153,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",1,46.888188026289463,{"$f":"F1768*(1-Elteq!$F$5)","v":46.888188026289463}]
["ANAMET-M",8242180,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 13-15,5 mm",1,44.110385723959254,{"$f":"F1769*(1-Elteq!$F$5)","v":44.110385723959254}]
["ANAMET-M",8242183,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 13-15,5 mm",1,46.888188026289463,{"$f":"F1770*(1-Elteq!$F$5)","v":46.888188026289463}]
["ANAMET-M",8242190,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15,5-18 mm",1,44.110385723959254,{"$f":"F1771*(1-Elteq!$F$5)","v":44.110385723959254}]
["ANAMET-M",8242193,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15,5-18 mm",1,46.888188026289463,{"$f":"F1772*(1-Elteq!$F$5)","v":46.888188026289463}]
["ANAMET-M",8242230,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15-18 mm",1,88.536641943835662,{"$f":"F1773*(1-Elteq!$F$5)","v":88.536641943835662}]
["ANAMET-M",8242233,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15-18 mm",1,92.53147468631721,{"$f":"F1774*(1-Elteq!$F$5)","v":92.53147468631721}]
["ANAMET-M",8242240,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 18-21 mm",1,88.536641943835662,{"$f":"F1775*(1-Elteq!$F$5)","v":88.536641943835662}]
["ANAMET-M",8242243,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 18-21 mm",1,92.53147468631721,{"$f":"F1776*(1-Elteq!$F$5)","v":92.53147468631721}]
["ANAMET-M",8242250,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-23,5 mm",1,88.536641943835662,{"$f":"F1777*(1-Elteq!$F$5)","v":88.536641943835662}]
["ANAMET-M",8242253,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-23,5 mm",1,92.53147468631721,{"$f":"F1778*(1-Elteq!$F$5)","v":92.53147468631721}]
["ANAMET-M",8220096,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",1,118.76730646484732,{"$f":"F1779*(1-Elteq!$F$5)","v":118.76730646484732}]
["ANAMET-M",8220099,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",1,116.57479361083419,{"$f":"F1780*(1-Elteq!$F$5)","v":116.57479361083419}]
["ANAMET-M",8220106,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",1,118.76730646484732,{"$f":"F1781*(1-Elteq!$F$5)","v":118.76730646484732}]
["ANAMET-M",8220109,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",1,116.57479361083419,{"$f":"F1782*(1-Elteq!$F$5)","v":116.57479361083419}]
["ANAMET-M",8220116,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 7-10 mm",1,118.76730646484732,{"$f":"F1783*(1-Elteq!$F$5)","v":118.76730646484732}]
["ANAMET-M",8220119,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 7-10 mm",1,116.57479361083419,{"$f":"F1784*(1-Elteq!$F$5)","v":116.57479361083419}]
["ANAMET-M",8220126,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 5,5-8 mm",1,157.11770079267038,{"$f":"F1785*(1-Elteq!$F$5)","v":157.11770079267038}]
["ANAMET-M",8220129,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 5,5-8 mm",1,155.55692893049152,{"$f":"F1786*(1-Elteq!$F$5)","v":155.55692893049152}]
["ANAMET-M",8220136,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 8-10,5 mm",1,157.11770079267038,{"$f":"F1787*(1-Elteq!$F$5)","v":157.11770079267038}]
["ANAMET-M",8220139,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 8-10,5 mm",1,155.55692893049152,{"$f":"F1788*(1-Elteq!$F$5)","v":155.55692893049152}]
["ANAMET-M",8220146,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",1,157.11770079267038,{"$f":"F1789*(1-Elteq!$F$5)","v":157.11770079267038}]
["ANAMET-M",8220149,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",1,155.55692893049152,{"$f":"F1790*(1-Elteq!$F$5)","v":155.55692893049152}]
["ANAMET-M",8220156,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",1,188.8533953236402,{"$f":"F1791*(1-Elteq!$F$5)","v":188.8533953236402}]
["ANAMET-M",8220159,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",1,186.15920579964103,{"$f":"F1792*(1-Elteq!$F$5)","v":186.15920579964103}]
["ANAMET-M",8220186,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 13-15,5 mm",1,188.8533953236402,{"$f":"F1793*(1-Elteq!$F$5)","v":188.8533953236402}]
["ANAMET-M",8220189,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 13-15,5 mm",1,186.15920579964103,{"$f":"F1794*(1-Elteq!$F$5)","v":186.15920579964103}]
["ANAMET-M",8220196,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15,5-18 mm",1,188.8533953236402,{"$f":"F1795*(1-Elteq!$F$5)","v":188.8533953236402}]
["ANAMET-M",8220199,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15,5-18 mm",1,186.15920579964103,{"$f":"F1796*(1-Elteq!$F$5)","v":186.15920579964103}]
["ANAMET-M",8220236,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15-18 mm",1,280.86461272256446,{"$f":"F1797*(1-Elteq!$F$5)","v":280.86461272256446}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8220239,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15-18 mm",1,276.99055399322771,{"$f":"F1798*(1-Elteq!$F$5)","v":276.99055399322771}]
["ANAMET-M",8220246,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 18-21 mm",1,280.86461272256446,{"$f":"F1799*(1-Elteq!$F$5)","v":280.86461272256446}]
["ANAMET-M",8220249,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 18-21 mm",1,276.99055399322771,{"$f":"F1800*(1-Elteq!$F$5)","v":276.99055399322771}]
["ANAMET-M",8220256,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-23,5 mm",1,280.86461272256446,{"$f":"F1801*(1-Elteq!$F$5)","v":280.86461272256446}]
["ANAMET-M",8220259,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-23,5 mm",1,276.99055399322771,{"$f":"F1802*(1-Elteq!$F$5)","v":276.99055399322771}]
["ANAMET-M",8220296,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-24 mm",1,430.50361500896122,{"$f":"F1803*(1-Elteq!$F$5)","v":430.50361500896122}]
["ANAMET-M",8220299,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-24 mm",1,421.42698340569495,{"$f":"F1804*(1-Elteq!$F$5)","v":421.42698340569495}]
["ANAMET-M",8220306,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 24-27 mm",1,430.50361500896122,{"$f":"F1805*(1-Elteq!$F$5)","v":430.50361500896122}]
["ANAMET-M",8220309,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 24-27 mm",1,421.42698340569495,{"$f":"F1806*(1-Elteq!$F$5)","v":421.42698340569495}]
["ANAMET-M",8220316,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 27-30 mm",1,430.50361500896122,{"$f":"F1807*(1-Elteq!$F$5)","v":430.50361500896122}]
["ANAMET-M",8220319,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 27-30 mm",1,421.42698340569495,{"$f":"F1808*(1-Elteq!$F$5)","v":421.42698340569495}]
["ANAMET-M",8240106,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",1,118.76730646484732,{"$f":"F1809*(1-Elteq!$F$5)","v":118.76730646484732}]
["ANAMET-M",8240109,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",1,116.57479361083419,{"$f":"F1810*(1-Elteq!$F$5)","v":116.57479361083419}]
["ANAMET-M",8240116,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 7-10 mm",1,118.76730646484732,{"$f":"F1811*(1-Elteq!$F$5)","v":118.76730646484732}]
["ANAMET-M",8240119,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 7-10 mm",1,116.57479361083419,{"$f":"F1812*(1-Elteq!$F$5)","v":116.57479361083419}]
["ANAMET-M",8240126,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 5,5-8 mm",1,157.11770079267038,{"$f":"F1813*(1-Elteq!$F$5)","v":157.11770079267038}]
["ANAMET-M",8240129,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 5,5-8 mm",1,155.55692893049152,{"$f":"F1814*(1-Elteq!$F$5)","v":155.55692893049152}]
["ANAMET-M",8240136,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 8-10,5 mm",1,157.11770079267038,{"$f":"F1815*(1-Elteq!$F$5)","v":157.11770079267038}]
["ANAMET-M",8240139,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 8-10,5 mm",1,155.55692893049152,{"$f":"F1816*(1-Elteq!$F$5)","v":155.55692893049152}]
["ANAMET-M",8240146,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",1,157.11770079267038,{"$f":"F1817*(1-Elteq!$F$5)","v":157.11770079267038}]
["ANAMET-M",8240149,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",1,155.55692893049152,{"$f":"F1818*(1-Elteq!$F$5)","v":155.55692893049152}]
["ANAMET-M",8240156,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",1,188.8533953236402,{"$f":"F1819*(1-Elteq!$F$5)","v":188.8533953236402}]
["ANAMET-M",8240159,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",1,186.15920579964103,{"$f":"F1820*(1-Elteq!$F$5)","v":186.15920579964103}]
["ANAMET-M",8240186,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 13-15,5 mm",1,188.8533953236402,{"$f":"F1821*(1-Elteq!$F$5)","v":188.8533953236402}]
["ANAMET-M",8240189,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 13-15,5 mm",1,186.15920579964103,{"$f":"F1822*(1-Elteq!$F$5)","v":186.15920579964103}]
["ANAMET-M",8240196,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15,5-18 mm",1,188.8533953236402,{"$f":"F1823*(1-Elteq!$F$5)","v":188.8533953236402}]
["ANAMET-M",8240199,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15,5-18 mm",1,186.15920579964103,{"$f":"F1824*(1-Elteq!$F$5)","v":186.15920579964103}]
["ANAMET-M",8240236,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15-18 mm",1,280.86461272256446,{"$f":"F1825*(1-Elteq!$F$5)","v":280.86461272256446}]
["ANAMET-M",8240239,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15-18 mm",1,276.99055399322771,{"$f":"F1826*(1-Elteq!$F$5)","v":276.99055399322771}]
["ANAMET-M",8240246,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 18-21 mm",1,280.86461272256446,{"$f":"F1827*(1-Elteq!$F$5)","v":280.86461272256446}]
["ANAMET-M",8240249,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 18-21 mm",1,276.99055399322771,{"$f":"F1828*(1-Elteq!$F$5)","v":276.99055399322771}]
["ANAMET-M",8240256,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-23,5 mm",1,280.86461272256446,{"$f":"F1829*(1-Elteq!$F$5)","v":280.86461272256446}]
["ANAMET-M",8240259,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-23,5 mm",1,276.99055399322771,{"$f":"F1830*(1-Elteq!$F$5)","v":276.99055399322771}]
["ANAMET-M",8222096,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",1,119.76136949611599,{"$f":"F1831*(1-Elteq!$F$5)","v":119.76136949611599}]
["ANAMET-M",8222099,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",1,117.58743725950973,{"$f":"F1832*(1-Elteq!$F$5)","v":117.58743725950973}]
["ANAMET-M",8222106,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",1,119.76136949611599,{"$f":"F1833*(1-Elteq!$F$5)","v":119.76136949611599}]
["ANAMET-M",8222109,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",1,117.58743725950973,{"$f":"F1834*(1-Elteq!$F$5)","v":117.58743725950973}]
["ANAMET-M",8222116,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 7-10 mm",1,119.76136949611599,{"$f":"F1835*(1-Elteq!$F$5)","v":119.76136949611599}]
["ANAMET-M",8222119,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 7-10 mm",1,117.58743725950973,{"$f":"F1836*(1-Elteq!$F$5)","v":117.58743725950973}]
["ANAMET-M",8222126,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 5,5-8 mm",1,158.3068603067114,{"$f":"F1837*(1-Elteq!$F$5)","v":158.3068603067114}]
["ANAMET-M",8222129,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 5,5-8 mm",1,156.74608844453255,{"$f":"F1838*(1-Elteq!$F$5)","v":156.74608844453255}]
["ANAMET-M",8222136,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 8-10,5 mm",1,158.3068603067114,{"$f":"F1839*(1-Elteq!$F$5)","v":158.3068603067114}]
["ANAMET-M",8222139,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 8-10,5 mm",1,156.74608844453255,{"$f":"F1840*(1-Elteq!$F$5)","v":156.74608844453255}]
["ANAMET-M",8222146,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",1,158.3068603067114,{"$f":"F1841*(1-Elteq!$F$5)","v":158.3068603067114}]
["ANAMET-M",8222149,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",1,156.74608844453255,{"$f":"F1842*(1-Elteq!$F$5)","v":156.74608844453255}]
["ANAMET-M",8222156,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",1,190.41416718581905,{"$f":"F1843*(1-Elteq!$F$5)","v":190.41416718581905}]
["ANAMET-M",8222159,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",1,187.71997766181985,{"$f":"F1844*(1-Elteq!$F$5)","v":187.71997766181985}]
["ANAMET-M",8222186,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 13-15,5 mm",1,190.41416718581905,{"$f":"F1845*(1-Elteq!$F$5)","v":190.41416718581905}]
["ANAMET-M",8222189,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 13-15,5 mm",1,187.71997766181985,{"$f":"F1846*(1-Elteq!$F$5)","v":187.71997766181985}]
["ANAMET-M",8222196,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15,5-18 mm",1,190.41416718581905,{"$f":"F1847*(1-Elteq!$F$5)","v":190.41416718581905}]
["ANAMET-M",8222199,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15,5-18 mm",1,187.71997766181985,{"$f":"F1848*(1-Elteq!$F$5)","v":187.71997766181985}]
["ANAMET-M",8222236,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15-18 mm",1,282.42538458474331,{"$f":"F1849*(1-Elteq!$F$5)","v":282.42538458474331}]
["ANAMET-M",8222239,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15-18 mm",1,278.55132585540656,{"$f":"F1850*(1-Elteq!$F$5)","v":278.55132585540656}]
["ANAMET-M",8222246,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 18-21 mm",1,282.42538458474331,{"$f":"F1851*(1-Elteq!$F$5)","v":282.42538458474331}]
["ANAMET-M",8222249,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 18-21 mm",1,278.55132585540656,{"$f":"F1852*(1-Elteq!$F$5)","v":278.55132585540656}]
["ANAMET-M",8222256,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-23,5 mm",1,282.42538458474331,{"$f":"F1853*(1-Elteq!$F$5)","v":282.42538458474331}]
["ANAMET-M",8222259,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-23,5 mm",1,278.55132585540656,{"$f":"F1854*(1-Elteq!$F$5)","v":278.55132585540656}]
["ANAMET-M",8222296,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-24 mm",1,433.44864286795348,{"$f":"F1855*(1-Elteq!$F$5)","v":433.44864286795348}]
["ANAMET-M",8222299,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-24 mm",1,424.37201126468716,{"$f":"F1856*(1-Elteq!$F$5)","v":424.37201126468716}]
["ANAMET-M",8222306,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 24-27 mm",1,433.44864286795348,{"$f":"F1857*(1-Elteq!$F$5)","v":433.44864286795348}]
["ANAMET-M",8222309,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 24-27 mm",1,424.37201126468716,{"$f":"F1858*(1-Elteq!$F$5)","v":424.37201126468716}]
["ANAMET-M",8222316,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 27-30 mm",1,433.44864286795348,{"$f":"F1859*(1-Elteq!$F$5)","v":433.44864286795348}]
["ANAMET-M",8222319,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 27-30 mm",1,424.37201126468716,{"$f":"F1860*(1-Elteq!$F$5)","v":424.37201126468716}]
["ANAMET-M",8242106,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",1,119.76136949611599,{"$f":"F1861*(1-Elteq!$F$5)","v":119.76136949611599}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8242109,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",1,117.58743725950973,{"$f":"F1862*(1-Elteq!$F$5)","v":117.58743725950973}]
["ANAMET-M",8242116,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 7-10 mm",1,119.76136949611599,{"$f":"F1863*(1-Elteq!$F$5)","v":119.76136949611599}]
["ANAMET-M",8242119,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 7-10 mm",1,117.58743725950973,{"$f":"F1864*(1-Elteq!$F$5)","v":117.58743725950973}]
["ANAMET-M",8242126,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 5,5-8 mm",1,158.3068603067114,{"$f":"F1865*(1-Elteq!$F$5)","v":158.3068603067114}]
["ANAMET-M",8242129,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 5,5-8 mm",1,156.74608844453255,{"$f":"F1866*(1-Elteq!$F$5)","v":156.74608844453255}]
["ANAMET-M",8242136,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 8-10,5 mm",1,158.3068603067114,{"$f":"F1867*(1-Elteq!$F$5)","v":158.3068603067114}]
["ANAMET-M",8242139,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 8-10,5 mm",1,156.74608844453255,{"$f":"F1868*(1-Elteq!$F$5)","v":156.74608844453255}]
["ANAMET-M",8242146,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",1,158.3068603067114,{"$f":"F1869*(1-Elteq!$F$5)","v":158.3068603067114}]
["ANAMET-M",8242149,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",1,156.74608844453255,{"$f":"F1870*(1-Elteq!$F$5)","v":156.74608844453255}]
["ANAMET-M",8242156,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",1,190.41416718581905,{"$f":"F1871*(1-Elteq!$F$5)","v":190.41416718581905}]
["ANAMET-M",8242159,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",1,187.71997766181985,{"$f":"F1872*(1-Elteq!$F$5)","v":187.71997766181985}]
["ANAMET-M",8242186,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 13-15,5 mm",1,190.41416718581905,{"$f":"F1873*(1-Elteq!$F$5)","v":190.41416718581905}]
["ANAMET-M",8242189,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 13-15,5 mm",1,187.71997766181985,{"$f":"F1874*(1-Elteq!$F$5)","v":187.71997766181985}]
["ANAMET-M",8242196,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15,5-18 mm",1,190.41416718581905,{"$f":"F1875*(1-Elteq!$F$5)","v":190.41416718581905}]
["ANAMET-M",8242199,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15,5-18 mm",1,187.71997766181985,{"$f":"F1876*(1-Elteq!$F$5)","v":187.71997766181985}]
["ANAMET-M",8242236,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15-18 mm",1,282.42538458474331,{"$f":"F1877*(1-Elteq!$F$5)","v":282.42538458474331}]
["ANAMET-M",8242239,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15-18 mm",1,278.55132585540656,{"$f":"F1878*(1-Elteq!$F$5)","v":278.55132585540656}]
["ANAMET-M",8242246,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 18-21 mm",1,282.42538458474331,{"$f":"F1879*(1-Elteq!$F$5)","v":282.42538458474331}]
["ANAMET-M",8242249,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 18-21 mm",1,278.55132585540656,{"$f":"F1880*(1-Elteq!$F$5)","v":278.55132585540656}]
["ANAMET-M",8242256,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-23,5 mm",1,282.42538458474331,{"$f":"F1881*(1-Elteq!$F$5)","v":282.42538458474331}]
["ANAMET-M",8242259,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-23,5 mm",1,278.55132585540656,{"$f":"F1882*(1-Elteq!$F$5)","v":278.55132585540656}]
["ANAMET-M",8223090,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",1,54.571273324038891,{"$f":"F1883*(1-Elteq!$F$5)","v":54.571273324038891}]
["ANAMET-M",8223093,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",1,56.187787038438401,{"$f":"F1884*(1-Elteq!$F$5)","v":56.187787038438401}]
["ANAMET-M",8223100,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",1,53.344952575184081,{"$f":"F1885*(1-Elteq!$F$5)","v":53.344952575184081}]
["ANAMET-M",8223103,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",1,55.611787898824787,{"$f":"F1886*(1-Elteq!$F$5)","v":55.611787898824787}]
["ANAMET-M",8223110,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 7-10 mm",1,53.344952575184081,{"$f":"F1887*(1-Elteq!$F$5)","v":53.344952575184081}]
["ANAMET-M",8223113,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 7-10 mm",1,55.611787898824787,{"$f":"F1888*(1-Elteq!$F$5)","v":55.611787898824787}]
["ANAMET-M",8223120,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 5,5-8 mm",1,57.869332913762044,{"$f":"F1889*(1-Elteq!$F$5)","v":57.869332913762044}]
["ANAMET-M",8223123,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 5,5-8 mm",1,59.485846628161568,{"$f":"F1890*(1-Elteq!$F$5)","v":59.485846628161568}]
["ANAMET-M",8223130,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 8-10,5 mm",1,57.869332913762044,{"$f":"F1891*(1-Elteq!$F$5)","v":57.869332913762044}]
["ANAMET-M",8223133,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 8-10,5 mm",1,59.485846628161568,{"$f":"F1892*(1-Elteq!$F$5)","v":59.485846628161568}]
["ANAMET-M",8223140,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",1,57.869332913762044,{"$f":"F1893*(1-Elteq!$F$5)","v":57.869332913762044}]
["ANAMET-M",8223143,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",1,59.485846628161568,{"$f":"F1894*(1-Elteq!$F$5)","v":59.485846628161568}]
["ANAMET-M",8223150,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",1,67.707769830710831,{"$f":"F1895*(1-Elteq!$F$5)","v":67.707769830710831}]
["ANAMET-M",8223153,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",1,70.355507811192808,{"$f":"F1896*(1-Elteq!$F$5)","v":70.355507811192808}]
["ANAMET-M",8223180,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 13-15,5 mm",1,67.707769830710831,{"$f":"F1897*(1-Elteq!$F$5)","v":67.707769830710831}]
["ANAMET-M",8223183,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 13-15,5 mm",1,70.355507811192808,{"$f":"F1898*(1-Elteq!$F$5)","v":70.355507811192808}]
["ANAMET-M",8223190,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15,5-18 mm",1,67.707769830710831,{"$f":"F1899*(1-Elteq!$F$5)","v":67.707769830710831}]
["ANAMET-M",8223193,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15,5-18 mm",1,70.355507811192808,{"$f":"F1900*(1-Elteq!$F$5)","v":70.355507811192808}]
["ANAMET-M",8223230,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15-18 mm",1,123.79336347341135,{"$f":"F1901*(1-Elteq!$F$5)","v":123.79336347341135}]
["ANAMET-M",8223233,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15-18 mm",1,127.74174467237569,{"$f":"F1902*(1-Elteq!$F$5)","v":127.74174467237569}]
["ANAMET-M",8223240,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 18-21 mm",1,123.79336347341135,{"$f":"F1903*(1-Elteq!$F$5)","v":123.79336347341135}]
["ANAMET-M",8223243,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 18-21 mm",1,127.74174467237569,{"$f":"F1904*(1-Elteq!$F$5)","v":127.74174467237569}]
["ANAMET-M",8223250,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-23,5 mm",1,123.79336347341135,{"$f":"F1905*(1-Elteq!$F$5)","v":123.79336347341135}]
["ANAMET-M",8223253,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-23,5 mm",1,127.74174467237569,{"$f":"F1906*(1-Elteq!$F$5)","v":127.74174467237569}]
["ANAMET-M",8223290,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-24 mm",1,168.87551548775102,{"$f":"F1907*(1-Elteq!$F$5)","v":168.87551548775102}]
["ANAMET-M",8223293,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-24 mm",1,178.18812093208479,{"$f":"F1908*(1-Elteq!$F$5)","v":178.18812093208479}]
["ANAMET-M",8223300,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 24-27 mm",1,168.87551548775102,{"$f":"F1909*(1-Elteq!$F$5)","v":168.87551548775102}]
["ANAMET-M",8223303,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 24-27 mm",1,178.18812093208479,{"$f":"F1910*(1-Elteq!$F$5)","v":178.18812093208479}]
["ANAMET-M",8223310,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 27-30 mm",1,168.87551548775102,{"$f":"F1911*(1-Elteq!$F$5)","v":168.87551548775102}]
["ANAMET-M",8223313,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 27-30 mm",1,178.18812093208479,{"$f":"F1912*(1-Elteq!$F$5)","v":178.18812093208479}]
["ANAMET-M",8243090,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",1,54.571273324038891,{"$f":"F1913*(1-Elteq!$F$5)","v":54.571273324038891}]
["ANAMET-M",8243093,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",1,56.187787038438401,{"$f":"F1914*(1-Elteq!$F$5)","v":56.187787038438401}]
["ANAMET-M",8243100,"NPT 3/8\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",1,53.344952575184081,{"$f":"F1915*(1-Elteq!$F$5)","v":53.344952575184081}]
["ANAMET-M",8243103,"NPT 3/8\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",1,55.611787898824787,{"$f":"F1916*(1-Elteq!$F$5)","v":55.611787898824787}]
["ANAMET-M",8243110,"NPT 3/8\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 7-10 mm",1,53.344952575184081,{"$f":"F1917*(1-Elteq!$F$5)","v":53.344952575184081}]
["ANAMET-M",8243113,"NPT 3/8\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 7-10 mm",1,55.611787898824787,{"$f":"F1918*(1-Elteq!$F$5)","v":55.611787898824787}]
["ANAMET-M",8243120,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 5,5-8 mm",1,57.869332913762044,{"$f":"F1919*(1-Elteq!$F$5)","v":57.869332913762044}]
["ANAMET-M",8243123,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 5,5-8 mm",1,59.485846628161568,{"$f":"F1920*(1-Elteq!$F$5)","v":59.485846628161568}]
["ANAMET-M",8243130,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 8-10,5 mm",1,57.869332913762044,{"$f":"F1921*(1-Elteq!$F$5)","v":57.869332913762044}]
["ANAMET-M",8243133,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 8-10,5 mm",1,59.485846628161568,{"$f":"F1922*(1-Elteq!$F$5)","v":59.485846628161568}]
["ANAMET-M",8243140,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",1,57.869332913762044,{"$f":"F1923*(1-Elteq!$F$5)","v":57.869332913762044}]
["ANAMET-M",8243143,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",1,59.485846628161568,{"$f":"F1924*(1-Elteq!$F$5)","v":59.485846628161568}]
["ANAMET-M",8243150,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",1,67.707769830710831,{"$f":"F1925*(1-Elteq!$F$5)","v":67.707769830710831}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8243153,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",1,70.355507811192808,{"$f":"F1926*(1-Elteq!$F$5)","v":70.355507811192808}]
["ANAMET-M",8243180,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 13-15,5 mm",1,67.707769830710831,{"$f":"F1927*(1-Elteq!$F$5)","v":67.707769830710831}]
["ANAMET-M",8243183,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 13-15,5 mm",1,70.355507811192808,{"$f":"F1928*(1-Elteq!$F$5)","v":70.355507811192808}]
["ANAMET-M",8243190,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15,5-18 mm",1,67.707769830710831,{"$f":"F1929*(1-Elteq!$F$5)","v":67.707769830710831}]
["ANAMET-M",8243193,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15,5-18 mm",1,70.355507811192808,{"$f":"F1930*(1-Elteq!$F$5)","v":70.355507811192808}]
["ANAMET-M",8243230,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15-18 mm",1,123.79336347341135,{"$f":"F1931*(1-Elteq!$F$5)","v":123.79336347341135}]
["ANAMET-M",8243233,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15-18 mm",1,127.74174467237569,{"$f":"F1932*(1-Elteq!$F$5)","v":127.74174467237569}]
["ANAMET-M",8243240,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 18-21 mm",1,123.79336347341135,{"$f":"F1933*(1-Elteq!$F$5)","v":123.79336347341135}]
["ANAMET-M",8243243,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 18-21 mm",1,127.74174467237569,{"$f":"F1934*(1-Elteq!$F$5)","v":127.74174467237569}]
["ANAMET-M",8243250,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-23,5 mm",1,123.79336347341135,{"$f":"F1935*(1-Elteq!$F$5)","v":123.79336347341135}]
["ANAMET-M",8243253,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-23,5 mm",1,127.74174467237569,{"$f":"F1936*(1-Elteq!$F$5)","v":127.74174467237569}]
["ANAMET-M",8223096,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",1,142.90352847639872,{"$f":"F1937*(1-Elteq!$F$5)","v":142.90352847639872}]
["ANAMET-M",8223099,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",1,140.69243500497871,{"$f":"F1938*(1-Elteq!$F$5)","v":140.69243500497871}]
["ANAMET-M",8223106,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",1,142.90352847639872,{"$f":"F1939*(1-Elteq!$F$5)","v":142.90352847639872}]
["ANAMET-M",8223109,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",1,140.69243500497871,{"$f":"F1940*(1-Elteq!$F$5)","v":140.69243500497871}]
["ANAMET-M",8223116,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 7-10 mm",1,142.90352847639872,{"$f":"F1941*(1-Elteq!$F$5)","v":142.90352847639872}]
["ANAMET-M",8223119,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 7-10 mm",1,140.69243500497871,{"$f":"F1942*(1-Elteq!$F$5)","v":140.69243500497871}]
["ANAMET-M",8223126,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 5,5-8 mm",1,181.55121268273203,{"$f":"F1943*(1-Elteq!$F$5)","v":181.55121268273203}]
["ANAMET-M",8223129,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 5,5-8 mm",1,179.98115051184973,{"$f":"F1944*(1-Elteq!$F$5)","v":179.98115051184973}]
["ANAMET-M",8223136,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 8-10,5 mm",1,181.55121268273203,{"$f":"F1945*(1-Elteq!$F$5)","v":181.55121268273203}]
["ANAMET-M",8223139,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 8-10,5 mm",1,179.98115051184973,{"$f":"F1946*(1-Elteq!$F$5)","v":179.98115051184973}]
["ANAMET-M",8223146,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",1,181.55121268273203,{"$f":"F1947*(1-Elteq!$F$5)","v":181.55121268273203}]
["ANAMET-M",8223149,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",1,179.98115051184973,{"$f":"F1948*(1-Elteq!$F$5)","v":179.98115051184973}]
["ANAMET-M",8223156,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",1,213.65851956183968,{"$f":"F1949*(1-Elteq!$F$5)","v":213.65851956183968}]
["ANAMET-M",8223159,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",1,211.08510405098531,{"$f":"F1950*(1-Elteq!$F$5)","v":211.08510405098531}]
["ANAMET-M",8223186,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 13-15,5 mm",1,213.65851956183968,{"$f":"F1951*(1-Elteq!$F$5)","v":213.65851956183968}]
["ANAMET-M",8223189,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 13-15,5 mm",1,211.08510405098531,{"$f":"F1952*(1-Elteq!$F$5)","v":211.08510405098531}]
["ANAMET-M",8223196,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15,5-18 mm",1,213.65851956183968,{"$f":"F1953*(1-Elteq!$F$5)","v":213.65851956183968}]
["ANAMET-M",8223199,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15,5-18 mm",1,211.08510405098531,{"$f":"F1954*(1-Elteq!$F$5)","v":211.08510405098531}]
["ANAMET-M",8223236,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15-18 mm",1,317.50559024895352,{"$f":"F1955*(1-Elteq!$F$5)","v":317.50559024895352}]
["ANAMET-M",8223239,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15-18 mm",1,313.67798306313398,{"$f":"F1956*(1-Elteq!$F$5)","v":313.67798306313398}]
["ANAMET-M",8223246,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 18-21 mm",1,317.50559024895352,{"$f":"F1957*(1-Elteq!$F$5)","v":317.50559024895352}]
["ANAMET-M",8223249,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 18-21 mm",1,313.67798306313398,{"$f":"F1958*(1-Elteq!$F$5)","v":313.67798306313398}]
["ANAMET-M",8223256,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-23,5 mm",1,317.50559024895352,{"$f":"F1959*(1-Elteq!$F$5)","v":317.50559024895352}]
["ANAMET-M",8223259,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-23,5 mm",1,313.67798306313398,{"$f":"F1960*(1-Elteq!$F$5)","v":313.67798306313398}]
["ANAMET-M",8223296,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-24 mm",1,471.91981120892132,{"$f":"F1961*(1-Elteq!$F$5)","v":471.91981120892132}]
["ANAMET-M",8223299,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-24 mm",1,462.88034084046876,{"$f":"F1962*(1-Elteq!$F$5)","v":462.88034084046876}]
["ANAMET-M",8223306,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 24-27 mm",1,471.91981120892132,{"$f":"F1963*(1-Elteq!$F$5)","v":471.91981120892132}]
["ANAMET-M",8223309,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 24-27 mm",1,462.88034084046876,{"$f":"F1964*(1-Elteq!$F$5)","v":462.88034084046876}]
["ANAMET-M",8223316,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 27-30 mm",1,471.91981120892132,{"$f":"F1965*(1-Elteq!$F$5)","v":471.91981120892132}]
["ANAMET-M",8223319,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 27-30 mm",1,462.88034084046876,{"$f":"F1966*(1-Elteq!$F$5)","v":462.88034084046876}]
["ANAMET-M",8243096,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",1,142.90352847639872,{"$f":"F1967*(1-Elteq!$F$5)","v":142.90352847639872}]
["ANAMET-M",8243099,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",1,140.69243500497871,{"$f":"F1968*(1-Elteq!$F$5)","v":140.69243500497871}]
["ANAMET-M",8243106,"NPT 3/8\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",1,142.90352847639872,{"$f":"F1969*(1-Elteq!$F$5)","v":142.90352847639872}]
["ANAMET-M",8243109,"NPT 3/8\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",1,140.69243500497871,{"$f":"F1970*(1-Elteq!$F$5)","v":140.69243500497871}]
["ANAMET-M",8243116,"NPT 3/8\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 7-10 mm",1,142.90352847639872,{"$f":"F1971*(1-Elteq!$F$5)","v":142.90352847639872}]
["ANAMET-M",8243119,"NPT 3/8\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 7-10 mm",1,140.69243500497871,{"$f":"F1972*(1-Elteq!$F$5)","v":140.69243500497871}]
["ANAMET-M",8243126,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 5,5-8 mm",1,181.55121268273203,{"$f":"F1973*(1-Elteq!$F$5)","v":181.55121268273203}]
["ANAMET-M",8243129,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 5,5-8 mm",1,179.98115051184973,{"$f":"F1974*(1-Elteq!$F$5)","v":179.98115051184973}]
["ANAMET-M",8243136,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 8-10,5 mm",1,181.55121268273203,{"$f":"F1975*(1-Elteq!$F$5)","v":181.55121268273203}]
["ANAMET-M",8243139,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 8-10,5 mm",1,179.98115051184973,{"$f":"F1976*(1-Elteq!$F$5)","v":179.98115051184973}]
["ANAMET-M",8243146,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",1,181.55121268273203,{"$f":"F1977*(1-Elteq!$F$5)","v":181.55121268273203}]
["ANAMET-M",8243149,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",1,179.98115051184973,{"$f":"F1978*(1-Elteq!$F$5)","v":179.98115051184973}]
["ANAMET-M",8243156,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",1,213.65851956183968,{"$f":"F1979*(1-Elteq!$F$5)","v":213.65851956183968}]
["ANAMET-M",8243159,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",1,211.08510405098531,{"$f":"F1980*(1-Elteq!$F$5)","v":211.08510405098531}]
["ANAMET-M",8243186,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 13-15,5 mm",1,213.65851956183968,{"$f":"F1981*(1-Elteq!$F$5)","v":213.65851956183968}]
["ANAMET-M",8243189,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 13-15,5 mm",1,211.08510405098531,{"$f":"F1982*(1-Elteq!$F$5)","v":211.08510405098531}]
["ANAMET-M",8243196,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15,5-18 mm",1,213.65851956183968,{"$f":"F1983*(1-Elteq!$F$5)","v":213.65851956183968}]
["ANAMET-M",8243199,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15,5-18 mm",1,211.08510405098531,{"$f":"F1984*(1-Elteq!$F$5)","v":211.08510405098531}]
["ANAMET-M",8243236,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15-18 mm",1,317.50559024895352,{"$f":"F1985*(1-Elteq!$F$5)","v":317.50559024895352}]
["ANAMET-M",8243239,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15-18 mm",1,313.67798306313398,{"$f":"F1986*(1-Elteq!$F$5)","v":313.67798306313398}]
["ANAMET-M",8243246,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 18-21 mm",1,317.50559024895352,{"$f":"F1987*(1-Elteq!$F$5)","v":317.50559024895352}]
["ANAMET-M",8243249,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 18-21 mm",1,313.67798306313398,{"$f":"F1988*(1-Elteq!$F$5)","v":313.67798306313398}]
["ANAMET-M",8243256,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-23,5 mm",1,317.50559024895352,{"$f":"F1989*(1-Elteq!$F$5)","v":317.50559024895352}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8243259,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-23,5 mm",1,313.67798306313398,{"$f":"F1990*(1-Elteq!$F$5)","v":313.67798306313398}]
["ANAMET-M",8261160,"M 16 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,43.710902449711092,{"$f":"F1991*(1-Elteq!$F$5)","v":43.710902449711092}]
["ANAMET-M",8261169,"M 16 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,176.2557367217681,{"$f":"F1992*(1-Elteq!$F$5)","v":176.2557367217681}]
["ANAMET-M",8261200,"M 20 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,43.710902449711092,{"$f":"F1993*(1-Elteq!$F$5)","v":43.710902449711092}]
["ANAMET-M",8261209,"M 20 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,176.2557367217681,{"$f":"F1994*(1-Elteq!$F$5)","v":176.2557367217681}]
["ANAMET-M",8261250,"M 25 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,55.630368516231684,{"$f":"F1995*(1-Elteq!$F$5)","v":55.630368516231684}]
["ANAMET-M",8261259,"M 25 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,243.57331358693423,{"$f":"F1996*(1-Elteq!$F$5)","v":243.57331358693423}]
["ANAMET-M",8261320,"M 32 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,82.377167273451292,{"$f":"F1997*(1-Elteq!$F$5)","v":82.377167273451292}]
["ANAMET-M",8261329,"M 32 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,462.06279367456563,{"$f":"F1998*(1-Elteq!$F$5)","v":462.06279367456563}]
["ANAMET-M",8261400,"M 40 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,141.10120858793033,{"$f":"F1999*(1-Elteq!$F$5)","v":141.10120858793033}]
["ANAMET-M",8261409,"M 40 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,496.32545217287264,{"$f":"F2000*(1-Elteq!$F$5)","v":496.32545217287264}]
["ANAMET-M",8261500,"M 50 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,171.64774360485913,{"$f":"F2001*(1-Elteq!$F$5)","v":171.64774360485913}]
["ANAMET-M",8261509,"M 50 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,547.12486016331252,{"$f":"F2002*(1-Elteq!$F$5)","v":547.12486016331252}]
["ANAMET-M",8271120,"NPT 1/2\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,43.710902449711092,{"$f":"F2003*(1-Elteq!$F$5)","v":43.710902449711092}]
["ANAMET-M",8271129,"NPT 1/2\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,176.2557367217681,{"$f":"F2004*(1-Elteq!$F$5)","v":176.2557367217681}]
["ANAMET-M",8271160,"NPT 1/2\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,43.710902449711092,{"$f":"F2005*(1-Elteq!$F$5)","v":43.710902449711092}]
["ANAMET-M",8271169,"NPT 1/2\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,176.2557367217681,{"$f":"F2006*(1-Elteq!$F$5)","v":176.2557367217681}]
["ANAMET-M",8271200,"NPT 3/4\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,55.630368516231684,{"$f":"F2007*(1-Elteq!$F$5)","v":55.630368516231684}]
["ANAMET-M",8271209,"NPT 3/4\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,243.57331358693423,{"$f":"F2008*(1-Elteq!$F$5)","v":243.57331358693423}]
["ANAMET-M",8271260,"NPT 1\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,82.377167273451292,{"$f":"F2009*(1-Elteq!$F$5)","v":82.377167273451292}]
["ANAMET-M",8271269,"NPT 1\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,462.06279367456563,{"$f":"F2010*(1-Elteq!$F$5)","v":462.06279367456563}]
["ANAMET-M",8271350,"NPT 1.1/4\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,141.10120858793033,{"$f":"F2011*(1-Elteq!$F$5)","v":141.10120858793033}]
["ANAMET-M",8271359,"NPT 1.1/4\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,496.32545217287264,{"$f":"F2012*(1-Elteq!$F$5)","v":496.32545217287264}]
["ANAMET-M",8271400,"NPT 1.1/2\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,171.64774360485913,{"$f":"F2013*(1-Elteq!$F$5)","v":171.64774360485913}]
["ANAMET-M",8271409,"NPT 1.1/2\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,547.12486016331252,{"$f":"F2014*(1-Elteq!$F$5)","v":547.12486016331252}]
["ANAMET-M",8275110,"Pg 11","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,43.710902449711092,{"$f":"F2015*(1-Elteq!$F$5)","v":43.710902449711092}]
["ANAMET-M",8275119,"Pg 11","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,176.2557367217681,{"$f":"F2016*(1-Elteq!$F$5)","v":176.2557367217681}]
["ANAMET-M",8275130,"Pg 13,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,43.710902449711092,{"$f":"F2017*(1-Elteq!$F$5)","v":43.710902449711092}]
["ANAMET-M",8275139,"Pg 13,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,176.2557367217681,{"$f":"F2018*(1-Elteq!$F$5)","v":176.2557367217681}]
["ANAMET-M",8275160,"Pg 16","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,43.710902449711092,{"$f":"F2019*(1-Elteq!$F$5)","v":43.710902449711092}]
["ANAMET-M",8275169,"Pg 16","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,176.2557367217681,{"$f":"F2020*(1-Elteq!$F$5)","v":176.2557367217681}]
["ANAMET-M",8275210,"Pg 21","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,55.630368516231684,{"$f":"F2021*(1-Elteq!$F$5)","v":55.630368516231684}]
["ANAMET-M",8275219,"Pg 21","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,243.57331358693423,{"$f":"F2022*(1-Elteq!$F$5)","v":243.57331358693423}]
["ANAMET-M",8275290,"Pg 29","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,82.377167273451292,{"$f":"F2023*(1-Elteq!$F$5)","v":82.377167273451292}]
["ANAMET-M",8275299,"Pg 29","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,462.06279367456563,{"$f":"F2024*(1-Elteq!$F$5)","v":462.06279367456563}]
["ANAMET-M",8275360,"Pg 36","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,141.10120858793033,{"$f":"F2025*(1-Elteq!$F$5)","v":141.10120858793033}]
["ANAMET-M",8275369,"Pg 36","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",1,496.32545217287264,{"$f":"F2026*(1-Elteq!$F$5)","v":496.32545217287264}]
["ANAMET-M",2978120,"M20 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 5,5-8 mm",1,31.224727552280338,{"$f":"F2027*(1-Elteq!$F$5)","v":31.224727552280338}]
["ANAMET-M",2978130,"M20 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 8-10,5 mm",1,31.224727552280338,{"$f":"F2028*(1-Elteq!$F$5)","v":31.224727552280338}]
["ANAMET-M",2978140,"M20 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 10,5-13 mm",1,31.224727552280338,{"$f":"F2029*(1-Elteq!$F$5)","v":31.224727552280338}]
["ANAMET-M",2978150,"M25 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 10,5-13 mm",1,39.725360015932978,{"$f":"F2030*(1-Elteq!$F$5)","v":39.725360015932978}]
["ANAMET-M",2978180,"M25 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 13-15,5 mm",1,39.725360015932978,{"$f":"F2031*(1-Elteq!$F$5)","v":39.725360015932978}]
["ANAMET-M",2978190,"M25 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 15,5-18 mm",1,39.725360015932978,{"$f":"F2032*(1-Elteq!$F$5)","v":39.725360015932978}]
["ANAMET-M",2978230,"M32 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 15-18 mm",1,58.835525018920379,{"$f":"F2033*(1-Elteq!$F$5)","v":58.835525018920379}]
["ANAMET-M",2978240,"M32 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 18-21 mm",1,58.835525018920379,{"$f":"F2034*(1-Elteq!$F$5)","v":58.835525018920379}]
["ANAMET-M",2978250,"M32 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 21-23,5 mm",1,58.835525018920379,{"$f":"F2035*(1-Elteq!$F$5)","v":58.835525018920379}]
["ANAMET-M",2978290,"M40 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 21-24 mm",1,100.79055912368027,{"$f":"F2036*(1-Elteq!$F$5)","v":100.79055912368027}]
["ANAMET-M",2978300,"M40 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 24-27 mm",1,100.79055912368027,{"$f":"F2037*(1-Elteq!$F$5)","v":100.79055912368027}]
["ANAMET-M",2978310,"M40 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 27-30 mm",1,100.79055912368027,{"$f":"F2038*(1-Elteq!$F$5)","v":100.79055912368027}]
["ANAMET-M",2979120,"NPT 1/2\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 5,5-8 mm",1,31.224727552280338,{"$f":"F2039*(1-Elteq!$F$5)","v":31.224727552280338}]
["ANAMET-M",2979130,"NPT 1/2\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 8-10,5 mm",1,31.224727552280338,{"$f":"F2040*(1-Elteq!$F$5)","v":31.224727552280338}]
["ANAMET-M",2979140,"NPT 1/2\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 10,5-13 mm",1,31.224727552280338,{"$f":"F2041*(1-Elteq!$F$5)","v":31.224727552280338}]
["ANAMET-M",2979150,"NPT 3/4\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 10,5-13 mm",1,39.725360015932978,{"$f":"F2042*(1-Elteq!$F$5)","v":39.725360015932978}]
["ANAMET-M",2979180,"NPT 3/4\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 13-15,5 mm",1,39.725360015932978,{"$f":"F2043*(1-Elteq!$F$5)","v":39.725360015932978}]
["ANAMET-M",2979190,"NPT 3/4\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 15,5-18 mm",1,39.725360015932978,{"$f":"F2044*(1-Elteq!$F$5)","v":39.725360015932978}]
["ANAMET-M",2979230,"NPT 1\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 15-18 mm",1,58.835525018920379,{"$f":"F2045*(1-Elteq!$F$5)","v":58.835525018920379}]
["ANAMET-M",2979240,"NPT 1\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 18-21 mm",1,58.835525018920379,{"$f":"F2046*(1-Elteq!$F$5)","v":58.835525018920379}]
["ANAMET-M",2979250,"NPT 1\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 21-23,5 mm",1,58.835525018920379,{"$f":"F2047*(1-Elteq!$F$5)","v":58.835525018920379}]
["ANAMET-M",2979290,"NPT 1 1/4\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 21-24 mm",1,100.79055912368027,{"$f":"F2048*(1-Elteq!$F$5)","v":100.79055912368027}]
["ANAMET-M",2979300,"NPT 1 1/4\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 24-27 mm",1,100.79055912368027,{"$f":"F2049*(1-Elteq!$F$5)","v":100.79055912368027}]
["ANAMET-M",2979310,"NPT 1 1/4\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 27-30 mm",1,100.79055912368027,{"$f":"F2050*(1-Elteq!$F$5)","v":100.79055912368027}]
["ANAMET-M",2976110,"PG 11","IEC-Ex ATEX fitting adapters, RNC fitting for cable 5,5-8 mm",1,31.224727552280338,{"$f":"F2051*(1-Elteq!$F$5)","v":31.224727552280338}]
["ANAMET-M",2976120,"PG 13,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 5,5-8 mm",1,31.224727552280338,{"$f":"F2052*(1-Elteq!$F$5)","v":31.224727552280338}]
["ANAMET-M",2976130,"PG 13,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 8-10,5 mm",1,31.224727552280338,{"$f":"F2053*(1-Elteq!$F$5)","v":31.224727552280338}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},2976140,"PG 13,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 10,5-13 mm",1,31.224727552280338,{"$f":"F2054*(1-Elteq!$F$5)","v":31.224727552280338}]
["ANAMET-M",2976150,"PG 16","IEC-Ex ATEX fitting adapters, RNC fitting for cable 10,5-13 mm",1,39.725360015932978,{"$f":"F2055*(1-Elteq!$F$5)","v":39.725360015932978}]
["ANAMET-M",2976180,"PG 16","IEC-Ex ATEX fitting adapters, RNC fitting for cable 13-15,5 mm",1,39.725360015932978,{"$f":"F2056*(1-Elteq!$F$5)","v":39.725360015932978}]
["ANAMET-M",2976190,"PG 16","IEC-Ex ATEX fitting adapters, RNC fitting for cable 15,5-18 mm",1,39.725360015932978,{"$f":"F2057*(1-Elteq!$F$5)","v":39.725360015932978}]
["ANAMET-M",2976230,"PG 21","IEC-Ex ATEX fitting adapters, RNC fitting for cable 15-18 mm",1,58.835525018920379,{"$f":"F2058*(1-Elteq!$F$5)","v":58.835525018920379}]
["ANAMET-M",2976240,"PG 21","IEC-Ex ATEX fitting adapters, RNC fitting for cable 18-21 mm",1,58.835525018920379,{"$f":"F2059*(1-Elteq!$F$5)","v":58.835525018920379}]
["ANAMET-M",2976250,"PG 21","IEC-Ex ATEX fitting adapters, RNC fitting for cable 21-23,5 mm",1,58.835525018920379,{"$f":"F2060*(1-Elteq!$F$5)","v":58.835525018920379}]
["ANAMET-M",2976290,"PG 29","IEC-Ex ATEX fitting adapters, RNC fitting for cable 21-24 mm",1,100.79055912368027,{"$f":"F2061*(1-Elteq!$F$5)","v":100.79055912368027}]
["ANAMET-M",2976300,"PG 29","IEC-Ex ATEX fitting adapters, RNC fitting for cable 24-27 mm",1,100.79055912368027,{"$f":"F2062*(1-Elteq!$F$5)","v":100.79055912368027}]
["ANAMET-M",2976310,"PG 29","IEC-Ex ATEX fitting adapters, RNC fitting for cable 27-30 mm",1,100.79055912368027,{"$f":"F2063*(1-Elteq!$F$5)","v":100.79055912368027}]
["ANAMET-M",8140401,"NPT 1.1/2\"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,31.670662370045729,{"$f":"F2064*(1-Elteq!$F$5)","v":31.670662370045729}]
["ANAMET-M",8140501,"NPT 2\"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,49.78676434176446,{"$f":"F2065*(1-Elteq!$F$5)","v":49.78676434176446}]
["ANAMET-M",8144111,"NPT 1/2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,10.107855869348709,{"$f":"F2066*(1-Elteq!$F$5)","v":10.107855869348709}]
["ANAMET-M",8144121,"NPT 1/2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,8.6864386377215457,{"$f":"F2067*(1-Elteq!$F$5)","v":8.6864386377215457}]
["ANAMET-M",8144161,"NPT 1/2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,9.281018394742059,{"$f":"F2068*(1-Elteq!$F$5)","v":9.281018394742059}]
["ANAMET-M",8144201,"NPT 3/4\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,12.560497367058321,{"$f":"F2069*(1-Elteq!$F$5)","v":12.560497367058321}]
["ANAMET-M",8144261,"NPT 1 \"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,23.1514492889862,{"$f":"F2070*(1-Elteq!$F$5)","v":23.1514492889862}]
["ANAMET-M",8194120,"NPT 1/2\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",1,15.951460043815931,{"$f":"F2071*(1-Elteq!$F$5)","v":15.951460043815931}]
["ANAMET-M",8194160,"NPT 1/2\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",1,20.773130260904146,{"$f":"F2072*(1-Elteq!$F$5)","v":20.773130260904146}]
["ANAMET-M",8194200,"NPT 3/4\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",1,29.682536307508382,{"$f":"F2073*(1-Elteq!$F$5)","v":29.682536307508382}]
["ANAMET-M",8194260,"NPT 1\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",1,47.306251917944508,{"$f":"F2074*(1-Elteq!$F$5)","v":47.306251917944508}]
["ANAMET-M",8199120,"NPT 1/2\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",1,15.951460043815931,{"$f":"F2075*(1-Elteq!$F$5)","v":15.951460043815931}]
["ANAMET-M",8199160,"NPT 1/2\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",1,20.773130260904146,{"$f":"F2076*(1-Elteq!$F$5)","v":20.773130260904146}]
["ANAMET-M",8199200,"NPT 3/4\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",1,29.682536307508382,{"$f":"F2077*(1-Elteq!$F$5)","v":29.682536307508382}]
["ANAMET-M",8199260,"NPT 1\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",1,47.306251917944508,{"$f":"F2078*(1-Elteq!$F$5)","v":47.306251917944508}]
["ANAMET-M",2978129,"M20 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 5,5-8 mm",1,125.89297324039002,{"$f":"F2079*(1-Elteq!$F$5)","v":125.89297324039002}]
["ANAMET-M",2978139,"M20 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 8-10,5 mm",1,125.89297324039002,{"$f":"F2080*(1-Elteq!$F$5)","v":125.89297324039002}]
["ANAMET-M",2978149,"M20 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 10,5-13 mm",1,125.89297324039002,{"$f":"F2081*(1-Elteq!$F$5)","v":125.89297324039002}]
["ANAMET-M",2978159,"M25 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 10,5-13 mm",1,173.97961108942397,{"$f":"F2082*(1-Elteq!$F$5)","v":173.97961108942397}]
["ANAMET-M",2978189,"M25 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 13-15,5 mm",1,173.97961108942397,{"$f":"F2083*(1-Elteq!$F$5)","v":173.97961108942397}]
["ANAMET-M",2978199,"M25 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 15,5-18 mm",1,173.97961108942397,{"$f":"F2084*(1-Elteq!$F$5)","v":173.97961108942397}]
["ANAMET-M",2978239,"M32 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 15-18 mm",1,331.05086033857708,{"$f":"F2085*(1-Elteq!$F$5)","v":331.05086033857708}]
["ANAMET-M",2978249,"M32 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 18-21 mm",1,331.05086033857708,{"$f":"F2086*(1-Elteq!$F$5)","v":331.05086033857708}]
["ANAMET-M",2978259,"M32 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 21-23,5 mm",1,331.05086033857708,{"$f":"F2087*(1-Elteq!$F$5)","v":331.05086033857708}]
["ANAMET-M",2978299,"M40 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 21-24 mm",1,354.51818012348048,{"$f":"F2088*(1-Elteq!$F$5)","v":354.51818012348048}]
["ANAMET-M",2978309,"M40 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 24-27 mm",1,354.51818012348048,{"$f":"F2089*(1-Elteq!$F$5)","v":354.51818012348048}]
["ANAMET-M",2978319,"M40 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 27-30 mm",1,354.51818012348048,{"$f":"F2090*(1-Elteq!$F$5)","v":354.51818012348048}]
["ANAMET-M",8140119,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,23.690287193786038,{"$f":"F2091*(1-Elteq!$F$5)","v":23.690287193786038}]
["ANAMET-M",8140129,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,22.268869962158874,{"$f":"F2092*(1-Elteq!$F$5)","v":22.268869962158874}]
["ANAMET-M",8140169,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,31.401243417645798,{"$f":"F2093*(1-Elteq!$F$5)","v":31.401243417645798}]
["ANAMET-M",8140209,"NPT 3/4\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,36.102139621589231,{"$f":"F2094*(1-Elteq!$F$5)","v":36.102139621589231}]
["ANAMET-M",8140269,"NPT 1 \"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,40.487165329615507,{"$f":"F2095*(1-Elteq!$F$5)","v":40.487165329615507}]
["ANAMET-M",8141129,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,30.407180386377131,{"$f":"F2096*(1-Elteq!$F$5)","v":30.407180386377131}]
["ANAMET-M",8141169,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,34.671432081258622,{"$f":"F2097*(1-Elteq!$F$5)","v":34.671432081258622}]
["ANAMET-M",8141209,"NPT 3/4\"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,51.626245465046672,{"$f":"F2098*(1-Elteq!$F$5)","v":51.626245465046672}]
["ANAMET-M",8141269,"NPT 1 \"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,68.961961505675987,{"$f":"F2099*(1-Elteq!$F$5)","v":68.961961505675987}]
["ANAMET-M",8192129,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67","1",58.696170388368699,{"$f":"F2100*(1-Elteq!$F$5)","v":58.696170388368699}]
["ANAMET-M",8192169,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67","1",77.035239768970129,{"$f":"F2101*(1-Elteq!$F$5)","v":77.035239768970129}]
["ANAMET-M",8195129,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67","1",58.696170388368699,{"$f":"F2102*(1-Elteq!$F$5)","v":58.696170388368699}]
["ANAMET-M",8195169,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67","1",77.035239768970129,{"$f":"F2103*(1-Elteq!$F$5)","v":77.035239768970129}]
["ANAMET-M",8382209,"NPT 3/4\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67",1,118.84162893447488,{"$f":"F2104*(1-Elteq!$F$5)","v":118.84162893447488}]
["ANAMET-M",8382269,"NPT 1\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67",1,182.52112091137175,{"$f":"F2105*(1-Elteq!$F$5)","v":182.52112091137175}]
["ANAMET-M",8385209,"NPT 3/4\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67",1,118.84162893447488,{"$f":"F2106*(1-Elteq!$F$5)","v":118.84162893447488}]
["ANAMET-M",8385269,"NPT 1\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67",1,182.52112091137175,{"$f":"F2107*(1-Elteq!$F$5)","v":182.52112091137175}]
["ANAMET-M",8140401,"NPT 1.1/2\"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,31.670662370045729,{"$f":"F2108*(1-Elteq!$F$5)","v":31.670662370045729}]
["ANAMET-M",8140501,"NPT 2\"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,49.78676434176446,{"$f":"F2109*(1-Elteq!$F$5)","v":49.78676434176446}]
["ANAMET-M",8144111,"NPT 1/2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,10.107855869348709,{"$f":"F2110*(1-Elteq!$F$5)","v":10.107855869348709}]
["ANAMET-M",8144121,"NPT 1/2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,8.6864386377215457,{"$f":"F2111*(1-Elteq!$F$5)","v":8.6864386377215457}]
["ANAMET-M",8144161,"NPT 1/2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,9.281018394742059,{"$f":"F2112*(1-Elteq!$F$5)","v":9.281018394742059}]
["ANAMET-M",8144201,"NPT 3/4\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,12.560497367058321,{"$f":"F2113*(1-Elteq!$F$5)","v":12.560497367058321}]
["ANAMET-M",8144261,"NPT 1 \"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,23.1514492889862,{"$f":"F2114*(1-Elteq!$F$5)","v":23.1514492889862}]
["ANAMET-M",8194120,"NPT 1/2\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",1,15.951460043815931,{"$f":"F2115*(1-Elteq!$F$5)","v":15.951460043815931}]
["ANAMET-M",8194160,"NPT 1/2\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",1,20.773130260904146,{"$f":"F2116*(1-Elteq!$F$5)","v":20.773130260904146}]
["ANAMET-M",8194200,"NPT 3/4\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",1,29.682536307508382,{"$f":"F2117*(1-Elteq!$F$5)","v":29.682536307508382}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8194260,"NPT 1\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",1,47.306251917944508,{"$f":"F2118*(1-Elteq!$F$5)","v":47.306251917944508}]
["ANAMET-M",8199120,"NPT 1/2\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",1,15.951460043815931,{"$f":"F2119*(1-Elteq!$F$5)","v":15.951460043815931}]
["ANAMET-M",8199160,"NPT 1/2\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",1,20.773130260904146,{"$f":"F2120*(1-Elteq!$F$5)","v":20.773130260904146}]
["ANAMET-M",8199200,"NPT 3/4\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",1,29.682536307508382,{"$f":"F2121*(1-Elteq!$F$5)","v":29.682536307508382}]
["ANAMET-M",8199260,"NPT 1\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",1,47.306251917944508,{"$f":"F2122*(1-Elteq!$F$5)","v":47.306251917944508}]
["ANAMET-M",8218120,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 5,5-8 mm",1,49.489474463254204,{"$f":"F2123*(1-Elteq!$F$5)","v":49.489474463254204}]
["ANAMET-M",8218130,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 8-10,5 mm",1,49.489474463254204,{"$f":"F2124*(1-Elteq!$F$5)","v":49.489474463254204}]
["ANAMET-M",8218140,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 10,5-13 mm",1,49.489474463254204,{"$f":"F2125*(1-Elteq!$F$5)","v":49.489474463254204}]
["ANAMET-M",8218150,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 10,5-13 mm",1,57.181850069707075,{"$f":"F2126*(1-Elteq!$F$5)","v":57.181850069707075}]
["ANAMET-M",8218180,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 13-15,5 mm",1,57.181850069707075,{"$f":"F2127*(1-Elteq!$F$5)","v":57.181850069707075}]
["ANAMET-M",8218190,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 15,5-18 mm",1,57.181850069707075,{"$f":"F2128*(1-Elteq!$F$5)","v":57.181850069707075}]
["ANAMET-M",8218230,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 15-18 mm",1,102.27700851623156,{"$f":"F2129*(1-Elteq!$F$5)","v":102.27700851623156}]
["ANAMET-M",8218240,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 18-21 mm",1,102.27700851623156,{"$f":"F2130*(1-Elteq!$F$5)","v":102.27700851623156}]
["ANAMET-M",8218250,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 21-23,5 mm",1,102.27700851623156,{"$f":"F2131*(1-Elteq!$F$5)","v":102.27700851623156}]
["ANAMET-M",8218290,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 21-24 mm",1,140.00495216092375,{"$f":"F2132*(1-Elteq!$F$5)","v":140.00495216092375}]
["ANAMET-M",8218300,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 24-27 mm",1,140.00495216092375,{"$f":"F2133*(1-Elteq!$F$5)","v":140.00495216092375}]
["ANAMET-M",8218310,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 27-30 mm",1,140.00495216092375,{"$f":"F2134*(1-Elteq!$F$5)","v":140.00495216092375}]
["ANAMET-M",8140119,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,23.690287193786038,{"$f":"F2135*(1-Elteq!$F$5)","v":23.690287193786038}]
["ANAMET-M",8140129,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,22.268869962158874,{"$f":"F2136*(1-Elteq!$F$5)","v":22.268869962158874}]
["ANAMET-M",8140169,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,31.401243417645798,{"$f":"F2137*(1-Elteq!$F$5)","v":31.401243417645798}]
["ANAMET-M",8140209,"NPT 3/4\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,36.102139621589231,{"$f":"F2138*(1-Elteq!$F$5)","v":36.102139621589231}]
["ANAMET-M",8140269,"NPT 1 \"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",1,40.487165329615507,{"$f":"F2139*(1-Elteq!$F$5)","v":40.487165329615507}]
["ANAMET-M",8141129,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,30.407180386377131,{"$f":"F2140*(1-Elteq!$F$5)","v":30.407180386377131}]
["ANAMET-M",8141169,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,34.671432081258622,{"$f":"F2141*(1-Elteq!$F$5)","v":34.671432081258622}]
["ANAMET-M",8141209,"NPT 3/4\"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,51.626245465046672,{"$f":"F2142*(1-Elteq!$F$5)","v":51.626245465046672}]
["ANAMET-M",8141269,"NPT 1 \"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,68.961961505675987,{"$f":"F2143*(1-Elteq!$F$5)","v":68.961961505675987}]
["ANAMET-M",8192129,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67","1",58.696170388368699,{"$f":"F2144*(1-Elteq!$F$5)","v":58.696170388368699}]
["ANAMET-M",8192169,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67","1",77.035239768970129,{"$f":"F2145*(1-Elteq!$F$5)","v":77.035239768970129}]
["ANAMET-M",8195129,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67","1",58.696170388368699,{"$f":"F2146*(1-Elteq!$F$5)","v":58.696170388368699}]
["ANAMET-M",8195169,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67","1",77.035239768970129,{"$f":"F2147*(1-Elteq!$F$5)","v":77.035239768970129}]
["ANAMET-M",8218129,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 5,5-8 mm",1,166.71458968332956,{"$f":"F2148*(1-Elteq!$F$5)","v":166.71458968332956}]
["ANAMET-M",8218139,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 8-10,5 mm",1,166.71458968332956,{"$f":"F2149*(1-Elteq!$F$5)","v":166.71458968332956}]
["ANAMET-M",8218149,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 10,5-13 mm",1,166.71458968332956,{"$f":"F2150*(1-Elteq!$F$5)","v":166.71458968332956}]
["ANAMET-M",8218159,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 10,5-13 mm",1,197.31686655247907,{"$f":"F2151*(1-Elteq!$F$5)","v":197.31686655247907}]
["ANAMET-M",8218189,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 13-15,5 mm",1,197.31686655247907,{"$f":"F2152*(1-Elteq!$F$5)","v":197.31686655247907}]
["ANAMET-M",8218199,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 15,5-18 mm",1,197.31686655247907,{"$f":"F2153*(1-Elteq!$F$5)","v":197.31686655247907}]
["ANAMET-M",8218239,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 15-18 mm",1,304.86148010356419,{"$f":"F2154*(1-Elteq!$F$5)","v":304.86148010356419}]
["ANAMET-M",8218249,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 18-21 mm",1,304.86148010356419,{"$f":"F2155*(1-Elteq!$F$5)","v":304.86148010356419}]
["ANAMET-M",8218259,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 21-23,5 mm",1,304.86148010356419,{"$f":"F2156*(1-Elteq!$F$5)","v":304.86148010356419}]
["ANAMET-M",8218299,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 21-24 mm",1,449.2979095160315,{"$f":"F2157*(1-Elteq!$F$5)","v":449.2979095160315}]
["ANAMET-M",8218309,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 24-27 mm",1,449.2979095160315,{"$f":"F2158*(1-Elteq!$F$5)","v":449.2979095160315}]
["ANAMET-M",8218319,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 27-30 mm",1,449.2979095160315,{"$f":"F2159*(1-Elteq!$F$5)","v":449.2979095160315}]
["ANAMET-M",8382209,"NPT 3/4\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67",1,118.84162893447488,{"$f":"F2160*(1-Elteq!$F$5)","v":118.84162893447488}]
["ANAMET-M",8382269,"NPT 1\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67",1,182.52112091137175,{"$f":"F2161*(1-Elteq!$F$5)","v":182.52112091137175}]
["ANAMET-M",8385209,"NPT 3/4\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67",1,118.84162893447488,{"$f":"F2162*(1-Elteq!$F$5)","v":118.84162893447488}]
["ANAMET-M",8385269,"NPT 1\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67",1,182.52112091137175,{"$f":"F2163*(1-Elteq!$F$5)","v":182.52112091137175}]
["ANAMET-M",8262160,"M 16 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",1,40.35710100776727,{"$f":"F2164*(1-Elteq!$F$5)","v":40.35710100776727}]
["ANAMET-M",8262169,"M 16 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",1,128.42922751643064,{"$f":"F2165*(1-Elteq!$F$5)","v":128.42922751643064}]
["ANAMET-M",8262200,"M 20 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",1,42.586775096594195,{"$f":"F2166*(1-Elteq!$F$5)","v":42.586775096594195}]
["ANAMET-M",8262209,"M 20 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",1,156.41163733120854,{"$f":"F2167*(1-Elteq!$F$5)","v":156.41163733120854}]
["ANAMET-M",8262250,"M 25 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",1,49.610248476398986,{"$f":"F2168*(1-Elteq!$F$5)","v":49.610248476398986}]
["ANAMET-M",8262259,"M 25 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",1,187.96152568810942,{"$f":"F2169*(1-Elteq!$F$5)","v":187.96152568810942}]
["ANAMET-M",8262320,"M 32 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",1,94.092246548496064,{"$f":"F2170*(1-Elteq!$F$5)","v":94.092246548496064}]
["ANAMET-M",8262329,"M 32 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",1,262.99005877713535,{"$f":"F2171*(1-Elteq!$F$5)","v":262.99005877713535}]
["ANAMET-M",8262400,"M 40 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",1,120.29091709221237,{"$f":"F2172*(1-Elteq!$F$5)","v":120.29091709221237}]
["ANAMET-M",8262409,"M 40 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",1,338.57601038836793,{"$f":"F2173*(1-Elteq!$F$5)","v":338.57601038836793}]
["ANAMET-M",8262500,"M 50 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",1,134.22638014738064,{"$f":"F2174*(1-Elteq!$F$5)","v":134.22638014738064}]
["ANAMET-M",8262509,"M 50 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",1,423.638076877115,{"$f":"F2175*(1-Elteq!$F$5)","v":423.638076877115}]
["ANAMET-M",8272160,"NPT 1/2\"","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",1,42.586775096594195,{"$f":"F2176*(1-Elteq!$F$5)","v":42.586775096594195}]
["ANAMET-M",8272169,"NPT 1/2\"","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",1,156.41163733120854,{"$f":"F2177*(1-Elteq!$F$5)","v":156.41163733120854}]
["ANAMET-M",8272200,"NPT 3/4\"","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",1,49.610248476398986,{"$f":"F2178*(1-Elteq!$F$5)","v":49.610248476398986}]
["ANAMET-M",8272209,"NPT 3/4\"","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",1,187.96152568810942,{"$f":"F2179*(1-Elteq!$F$5)","v":187.96152568810942}]
["ANAMET-M",8272260,"NPT 1\"","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",1,94.092246548496064,{"$f":"F2180*(1-Elteq!$F$5)","v":94.092246548496064}]
["ANAMET-M",8272269,"NPT 1\"","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",1,262.99005877713535,{"$f":"F2181*(1-Elteq!$F$5)","v":262.99005877713535}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8272350,"NPT 1.1/4\"","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",1,130.32445049193353,{"$f":"F2182*(1-Elteq!$F$5)","v":130.32445049193353}]
["ANAMET-M",8272359,"NPT 1.1/4\"","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",1,348.60954378808907,{"$f":"F2183*(1-Elteq!$F$5)","v":348.60954378808907}]
["ANAMET-M",8272400,"NPT 1.1/2\"","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",1,144.25991354710177,{"$f":"F2184*(1-Elteq!$F$5)","v":144.25991354710177}]
["ANAMET-M",8272409,"NPT 1.1/2\"","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",1,433.67161027683613,{"$f":"F2185*(1-Elteq!$F$5)","v":433.67161027683613}]
["ANAMET-M",7812200,"M 16 X 1,5","IEC-Ex ATEX fittings for Sealtite, Enlarger ISO/ISO nickel plated brass",1,30.06343896434965,{"$f":"F2186*(1-Elteq!$F$5)","v":30.06343896434965}]
["ANAMET-M",7812250,"M 20 X 1,5","IEC-Ex ATEX fittings for Sealtite, Enlarger ISO/ISO nickel plated brass",1,29.487439824736029,{"$f":"F2187*(1-Elteq!$F$5)","v":29.487439824736029}]
["ANAMET-M",7812320,"M 25 X 1,5","IEC-Ex ATEX fittings for Sealtite, Enlarger ISO/ISO nickel plated brass",1,35.507559864568712,{"$f":"F2188*(1-Elteq!$F$5)","v":35.507559864568712}]
["ANAMET-M",7822160,"M 20 X 1,5","IEC-Ex ATEX fittings for Sealtite, Reducer ISO/ISO nickel plated brass",1,30.06343896434965,{"$f":"F2189*(1-Elteq!$F$5)","v":30.06343896434965}]
["ANAMET-M",7822200,"M 25 X 1,5","IEC-Ex ATEX fittings for Sealtite, Reducer ISO/ISO nickel plated brass",1,27.341378514240116,{"$f":"F2190*(1-Elteq!$F$5)","v":27.341378514240116}]
["ANAMET-M",7822250,"M 32 X 1,5","IEC-Ex ATEX fittings for Sealtite, Reducer ISO/ISO nickel plated brass",1,33.231434232224572,{"$f":"F2191*(1-Elteq!$F$5)","v":33.231434232224572}]
["ANAMET-M",7822320,"M 40 X 1,5","IEC-Ex ATEX fittings for Sealtite, Reducer ISO/ISO nickel plated brass",1,42.038646883090905,{"$f":"F2192*(1-Elteq!$F$5)","v":42.038646883090905}]
["ANAMET-M",8801160,"M16 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,0.24154802628958311,{"$f":"F2193*(1-Elteq!$F$5)","v":0.24154802628958311}]
["ANAMET-M",8801200,"M20 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,0.3344511133240381,{"$f":"F2194*(1-Elteq!$F$5)","v":0.3344511133240381}]
["ANAMET-M",8801250,"M25 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,0.48309605257916621,{"$f":"F2195*(1-Elteq!$F$5)","v":0.48309605257916621}]
["ANAMET-M",8801320,"M32 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,0.60387006572395774,{"$f":"F2196*(1-Elteq!$F$5)","v":0.60387006572395774}]
["ANAMET-M",8801400,"M40 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,1.4957397012547262,{"$f":"F2197*(1-Elteq!$F$5)","v":1.4957397012547262}]
["ANAMET-M",8801500,"M50 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,2.4061899541923855,{"$f":"F2198*(1-Elteq!$F$5)","v":2.4061899541923855}]
["ANAMET-M",8801630,"M63 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,3.3909626767576091,{"$f":"F2199*(1-Elteq!$F$5)","v":3.3909626767576091}]
["ANAMET-M",8802160,"NPT 1/2\"","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,0.62245068313084884,{"$f":"F2200*(1-Elteq!$F$5)","v":0.62245068313084884}]
["ANAMET-M",8802200,"NPT 3/4\"","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,0.78967623979286783,{"$f":"F2201*(1-Elteq!$F$5)","v":0.78967623979286783}]
["ANAMET-M",8802260,"NPT 1 \"","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,1.3470947619995981,{"$f":"F2202*(1-Elteq!$F$5)","v":1.3470947619995981}]
["ANAMET-M",8802350,"NPT 1 1/4\"","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,1.9602551364270013,{"$f":"F2203*(1-Elteq!$F$5)","v":1.9602551364270013}]
["ANAMET-M",8802400,"NPT 1 1/2\"","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,3.455994837681728,{"$f":"F2204*(1-Elteq!$F$5)","v":3.455994837681728}]
["ANAMET-M",8802500,"NPT 2\"","Fitting accessories for Sealtite, Locknut, nickel plated brass",1,6.7261835012945452,{"$f":"F2205*(1-Elteq!$F$5)","v":6.7261835012945452}]
["ANAMET-M",8805100,"M16 x 1,5 / NPT 3/8\"","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",1,6.4660548575980705,{"$f":"F2206*(1-Elteq!$F$5)","v":6.4660548575980705}]
["ANAMET-M",8805110,"PG 11","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",1,6.4660548575980705,{"$f":"F2207*(1-Elteq!$F$5)","v":6.4660548575980705}]
["ANAMET-M",8805120,"M20  / PG13,5 / NPT1/2\"","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",1,6.4660548575980705,{"$f":"F2208*(1-Elteq!$F$5)","v":6.4660548575980705}]
["ANAMET-M",8805130,"M25 x 1,5  / NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",1,6.8562478231427821,{"$f":"F2209*(1-Elteq!$F$5)","v":6.8562478231427821}]
["ANAMET-M",8805160,"PG 16","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",1,6.8562478231427821,{"$f":"F2210*(1-Elteq!$F$5)","v":6.8562478231427821}]
["ANAMET-M",8805200,"M32 x 1,5 / NPT 1\"","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",1,9.1230831467834843,{"$f":"F2211*(1-Elteq!$F$5)","v":9.1230831467834843}]
["ANAMET-M",8805210,"PG 21","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",1,9.1230831467834843,{"$f":"F2212*(1-Elteq!$F$5)","v":9.1230831467834843}]
["ANAMET-M",8805250,"NPT 1.1/4”","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",1,12.216755945030839,{"$f":"F2213*(1-Elteq!$F$5)","v":12.216755945030839}]
["ANAMET-M",8805270,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",1,12.216755945030839,{"$f":"F2214*(1-Elteq!$F$5)","v":12.216755945030839}]
["ANAMET-M",8805290,"Pg 29","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",1,12.216755945030839,{"$f":"F2215*(1-Elteq!$F$5)","v":12.216755945030839}]
["ANAMET-M",8805320,"NPT 1.1/2”","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",1,15.133912877912726,{"$f":"F2216*(1-Elteq!$F$5)","v":15.133912877912726}]
["ANAMET-M",8805350,"M50 x 1,5","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",1,15.133912877912726,{"$f":"F2217*(1-Elteq!$F$5)","v":15.133912877912726}]
["ANAMET-M",8805360,"Pg 36","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",1,15.133912877912726,{"$f":"F2218*(1-Elteq!$F$5)","v":15.133912877912726}]
["ANAMET-M",8805420,"Pg 42","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",1,15.133912877912726,{"$f":"F2219*(1-Elteq!$F$5)","v":15.133912877912726}]
["ANAMET-M",7811110,"M 20 X 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/PG nickel plated brass",1,30.06343896434965,{"$f":"F2220*(1-Elteq!$F$5)","v":30.06343896434965}]
["ANAMET-M",7811150,"M 20 X 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/PG nickel plated brass",1,29.487439824736029,{"$f":"F2221*(1-Elteq!$F$5)","v":29.487439824736029}]
["ANAMET-M",7811160,"M 25 X 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/PG nickel plated brass",1,29.487439824736029,{"$f":"F2222*(1-Elteq!$F$5)","v":29.487439824736029}]
["ANAMET-M",7811180,"M 25 X 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/PG nickel plated brass",1,33.231434232224572,{"$f":"F2223*(1-Elteq!$F$5)","v":33.231434232224572}]
["ANAMET-M",7811210,"M 32 X 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/PG nickel plated brass",1,35.507559864568712,{"$f":"F2224*(1-Elteq!$F$5)","v":35.507559864568712}]
["ANAMET-M",7821110,"PG 11","IEC-Ex ATEX fittings for Sealtite, Adapter PG/ISO nickel plated brass",1,30.06343896434965,{"$f":"F2225*(1-Elteq!$F$5)","v":30.06343896434965}]
["ANAMET-M",7821160,"PG 16","IEC-Ex ATEX fittings for Sealtite, Adapter PG/ISO nickel plated brass",1,29.487439824736029,{"$f":"F2226*(1-Elteq!$F$5)","v":29.487439824736029}]
["ANAMET-M",7821210,"PG 21","IEC-Ex ATEX fittings for Sealtite, Adapter PG/ISO nickel plated brass",1,33.231434232224572,{"$f":"F2227*(1-Elteq!$F$5)","v":33.231434232224572}]
["ANAMET-M",7821290,"PG 29","IEC-Ex ATEX fittings for Sealtite, Adapter PG/ISO nickel plated brass",1,42.038646883090905,{"$f":"F2228*(1-Elteq!$F$5)","v":42.038646883090905}]
["ANAMET-M",7824110,"PG 11","IEC-Ex ATEX fittings for Sealtite, Adapter PG/NPT nickel plated brass",1,30.06343896434965,{"$f":"F2229*(1-Elteq!$F$5)","v":30.06343896434965}]
["ANAMET-M",7824120,"PG 11","IEC-Ex ATEX fittings for Sealtite, Adapter PG/NPT nickel plated brass",1,30.06343896434965,{"$f":"F2230*(1-Elteq!$F$5)","v":30.06343896434965}]
["ANAMET-M",7824130,"PG 13,5","IEC-Ex ATEX fittings for Sealtite, Adapter PG/NPT nickel plated brass",1,27.341378514240116,{"$f":"F2231*(1-Elteq!$F$5)","v":27.341378514240116}]
["ANAMET-M",7824160,"PG 16","IEC-Ex ATEX fittings for Sealtite, Adapter PG/NPT nickel plated brass",1,27.341378514240116,{"$f":"F2232*(1-Elteq!$F$5)","v":27.341378514240116}]
["ANAMET-M",7824200,"PG 21","IEC-Ex ATEX fittings for Sealtite, Adapter PG/NPT nickel plated brass",1,33.231434232224572,{"$f":"F2233*(1-Elteq!$F$5)","v":33.231434232224572}]
["ANAMET-M",7824260,"PG 29","IEC-Ex ATEX fittings for Sealtite, Adapter PG/NPT nickel plated brass",1,42.038646883090905,{"$f":"F2234*(1-Elteq!$F$5)","v":42.038646883090905}]
["ANAMET-M",7825160,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",1,30.06343896434965,{"$f":"F2235*(1-Elteq!$F$5)","v":30.06343896434965}]
["ANAMET-M",7825200,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",1,27.341378514240116,{"$f":"F2236*(1-Elteq!$F$5)","v":27.341378514240116}]
["ANAMET-M",7825220,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",1,29.487439824736029,{"$f":"F2237*(1-Elteq!$F$5)","v":29.487439824736029}]
["ANAMET-M",7825240,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",1,27.341378514240116,{"$f":"F2238*(1-Elteq!$F$5)","v":27.341378514240116}]
["ANAMET-M",7825250,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",1,29.487439824736029,{"$f":"F2239*(1-Elteq!$F$5)","v":29.487439824736029}]
["ANAMET-M",7825270,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",1,35.507559864568712,{"$f":"F2240*(1-Elteq!$F$5)","v":35.507559864568712}]
["ANAMET-M",7825280,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",1,33.231434232224572,{"$f":"F2241*(1-Elteq!$F$5)","v":33.231434232224572}]
["ANAMET-M",7825320,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",1,35.507559864568712,{"$f":"F2242*(1-Elteq!$F$5)","v":35.507559864568712}]
["ANAMET-M",7826120,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/NPT nickel plated brass",1,30.06343896434965,{"$f":"F2243*(1-Elteq!$F$5)","v":30.06343896434965}]
["ANAMET-M",7826160,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/NPT nickel plated brass",1,27.341378514240116,{"$f":"F2244*(1-Elteq!$F$5)","v":27.341378514240116}]
["ANAMET-M",7826180,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/NPT nickel plated brass",1,27.341378514240116,{"$f":"F2245*(1-Elteq!$F$5)","v":27.341378514240116}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},7826200,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/NPT nickel plated brass",1,29.487439824736029,{"$f":"F2246*(1-Elteq!$F$5)","v":29.487439824736029}]
["ANAMET-M",7826260,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/NPT nickel plated brass",1,35.507559864568712,{"$f":"F2247*(1-Elteq!$F$5)","v":35.507559864568712}]
["ANAMET-M",7813160,"M 16 x 1,5","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",1,6.921279984066901,{"$f":"F2248*(1-Elteq!$F$5)","v":6.921279984066901}]
["ANAMET-M",7813200,"M 20 x 1,5","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",1,8.0825685719975873,{"$f":"F2249*(1-Elteq!$F$5)","v":8.0825685719975873}]
["ANAMET-M",7813250,"M 25 x 1,5","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",1,12.727722923720341,{"$f":"F2250*(1-Elteq!$F$5)","v":12.727722923720341}]
["ANAMET-M",7813320,"M 32 x 1,5","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",1,23.532351945827461,{"$f":"F2251*(1-Elteq!$F$5)","v":23.532351945827461}]
["ANAMET-M",7814160,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",1,10.851080565624349,{"$f":"F2252*(1-Elteq!$F$5)","v":10.851080565624349}]
["ANAMET-M",7814200,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",1,13.638173176657999,{"$f":"F2253*(1-Elteq!$F$5)","v":13.638173176657999}]
["ANAMET-M",7814260,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",1,23.20719114120687,{"$f":"F2254*(1-Elteq!$F$5)","v":23.20719114120687}]
["ANAMET-M",7815110,"PG 11","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",1,8.5285033897629727,{"$f":"F2255*(1-Elteq!$F$5)","v":8.5285033897629727}]
["ANAMET-M",7815130,"PG 13,5","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",1,10.851080565624349,{"$f":"F2256*(1-Elteq!$F$5)","v":10.851080565624349}]
["ANAMET-M",7815160,"PG 16","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",1,13.638173176657999,{"$f":"F2257*(1-Elteq!$F$5)","v":13.638173176657999}]
["ANAMET-M",7815210,"PG 21","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",1,23.20719114120687,{"$f":"F2258*(1-Elteq!$F$5)","v":23.20719114120687}]
["ANAMET-M",7815290,"PG 29","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",1,32.971305588528097,{"$f":"F2259*(1-Elteq!$F$5)","v":32.971305588528097}]
["ANAMET-M",7817160,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/NPT male nickel plated brass",1,27.341378514240116,{"$f":"F2260*(1-Elteq!$F$5)","v":27.341378514240116}]
["ANAMET-M",7817200,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/NPT male nickel plated brass",1,29.487439824736029,{"$f":"F2261*(1-Elteq!$F$5)","v":29.487439824736029}]
["ANAMET-M",7817260,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/NPT male nickel plated brass",1,35.507559864568712,{"$f":"F2262*(1-Elteq!$F$5)","v":35.507559864568712}]
["ANAMET-M",7823110,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/PG nickel plated brass",1,30.06343896434965,{"$f":"F2263*(1-Elteq!$F$5)","v":30.06343896434965}]
["ANAMET-M",7823130,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/PG nickel plated brass",1,30.06343896434965,{"$f":"F2264*(1-Elteq!$F$5)","v":30.06343896434965}]
["ANAMET-M",7823160,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/PG nickel plated brass",1,29.487439824736029,{"$f":"F2265*(1-Elteq!$F$5)","v":29.487439824736029}]
["ANAMET-M",7823200,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/PG nickel plated brass",1,29.487439824736029,{"$f":"F2266*(1-Elteq!$F$5)","v":29.487439824736029}]
["ANAMET-M",7823210,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/PG nickel plated brass",1,35.507559864568712,{"$f":"F2267*(1-Elteq!$F$5)","v":35.507559864568712}]
["ANAMET-M",7823260,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/PG nickel plated brass",1,35.507559864568712,{"$f":"F2268*(1-Elteq!$F$5)","v":35.507559864568712}]
["ANAMET-M",7823290,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/PG nickel plated brass",1,46.432962899820623,{"$f":"F2269*(1-Elteq!$F$5)","v":46.432962899820623}]
["ANAMET-M",7827160,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/NPT fem nickel plated brass",1,27.341378514240116,{"$f":"F2270*(1-Elteq!$F$5)","v":27.341378514240116}]
["ANAMET-M",7827200,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/NPT fem nickel plated brass",1,29.487439824736029,{"$f":"F2271*(1-Elteq!$F$5)","v":29.487439824736029}]
["ANAMET-M",7827260,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/NPT fem nickel plated brass",1,35.507559864568712,{"$f":"F2272*(1-Elteq!$F$5)","v":35.507559864568712}]
["ANAMET-M",7829160,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, Fitting dus cap EPDM",1,7.0885055407289199,{"$f":"F2273*(1-Elteq!$F$5)","v":7.0885055407289199}]
["ANAMET-M",7829200,"M20 x 1,5 / NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, Fitting dus cap EPDM",1,7.5344403584943027,{"$f":"F2274*(1-Elteq!$F$5)","v":7.5344403584943027}]
["ANAMET-M",7829250,"M25 x 1,5 / NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, Fitting dus cap EPDM",1,8.1754716590320449,{"$f":"F2275*(1-Elteq!$F$5)","v":8.1754716590320449}]
["ANAMET-M",7829320,"M32 x 1,5 / NPT 1\"","IEC-Ex ATEX fittings for Sealtite, Fitting dus cap EPDM",1,10.367984513045183,{"$f":"F2276*(1-Elteq!$F$5)","v":10.367984513045183}]
["ANAMET-M",8279991,"50 gr","IEC-Ex ATEX fittings for Sealtite, Sealing compound for BXA/BXC/BXN",1,9.3088893208523942,{"$f":"F2277*(1-Elteq!$F$5)","v":9.3088893208523942}]
["ANAMET-M",8801168,"M16 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 316",1,16.945523075084598,{"$f":"F2278*(1-Elteq!$F$5)","v":16.945523075084598}]
["ANAMET-M",8801208,"M20 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 316",1,19.509648277235559,{"$f":"F2279*(1-Elteq!$F$5)","v":19.509648277235559}]
["ANAMET-M",8801258,"M25 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 316",1,23.355836080461998,{"$f":"F2280*(1-Elteq!$F$5)","v":23.355836080461998}]
["ANAMET-M",8801328,"M32 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 316",1,41.63916360884275,{"$f":"F2281*(1-Elteq!$F$5)","v":41.63916360884275}]
["ANAMET-M",8801408,"M40 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 316",1,57.302624082851864,{"$f":"F2282*(1-Elteq!$F$5)","v":57.302624082851864}]
["ANAMET-M",8802168,"NPT 1/2\"","Fitting accessories for Sealtite, Locknut, stainless steel 316",1,20.79171087831104,{"$f":"F2283*(1-Elteq!$F$5)","v":20.79171087831104}]
["ANAMET-M",8802208,"NPT 3/4\"","Fitting accessories for Sealtite, Locknut, stainless steel 316",1,24.693640533758149,{"$f":"F2284*(1-Elteq!$F$5)","v":24.693640533758149}]
["ANAMET-M",8802268,"NPT 1\"","Fitting accessories for Sealtite, Locknut, stainless steel 316",1,44.203288810993712,{"$f":"F2285*(1-Elteq!$F$5)","v":44.203288810993712}]
["ANAMET-M",8802358,"NPT 1.1/4\"","Fitting accessories for Sealtite, Locknut, stainless steel 316",1,59.866749285002825,{"$f":"F2286*(1-Elteq!$F$5)","v":59.866749285002825}]
["ANAMET-M",8802408,"NPT 1.1/2\"","Fitting accessories for Sealtite, Locknut, stainless steel 316",1,97.548241386177793,{"$f":"F2287*(1-Elteq!$F$5)","v":97.548241386177793}]
["ANAMET-M",2983120,"NPT 1/2\"","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",1,18.952229755028828,{"$f":"F2288*(1-Elteq!$F$5)","v":18.952229755028828}]
["ANAMET-M",2983160,"NPT 1/2\"","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",1,21.55351619199357,{"$f":"F2289*(1-Elteq!$F$5)","v":21.55351619199357}]
["ANAMET-M",2983200,"NPT 3/4\"","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",1,29.728987851025614,{"$f":"F2290*(1-Elteq!$F$5)","v":29.728987851025614}]
["ANAMET-M",2983260,"NPT 1\"","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",1,46.265737343158605,{"$f":"F2291*(1-Elteq!$F$5)","v":46.265737343158605}]
["ANAMET-M",2983350,"NPT 1 1/4\"","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",1,69.677315275841281,{"$f":"F2292*(1-Elteq!$F$5)","v":69.677315275841281}]
["ANAMET-M",2987120,"NPT 1/2\"","Sealtite fittings for CNP, 90° elbow fixed with male thread, IP 67",1,35.303173073092914,{"$f":"F2293*(1-Elteq!$F$5)","v":35.303173073092914}]
["ANAMET-M",2987160,"NPT 1/2\"","Sealtite fittings for CNP, 90° elbow fixed with male thread, IP 67",1,35.303173073092914,{"$f":"F2294*(1-Elteq!$F$5)","v":35.303173073092914}]
["ANAMET-M",2987200,"NPT 3/4\"","Sealtite fittings for CNP, 90° elbow fixed with male thread, IP 67",1,53.697984305915007,{"$f":"F2295*(1-Elteq!$F$5)","v":53.697984305915007}]
["ANAMET-M",2987260,"NPT 1\"","Sealtite fittings for CNP, 90° elbow fixed with male thread, IP 67",1,99.842947635928837,{"$f":"F2296*(1-Elteq!$F$5)","v":99.842947635928837}]
["ANAMET-M",2987350,"NPT 1 1/4\"","Sealtite fittings for CNP, 90° elbow fixed with male thread, IP 67",1,165.98065529575737,{"$f":"F2297*(1-Elteq!$F$5)","v":165.98065529575737}]
["ANAMET-M",8280169,"M 16 x 1,5","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",1,47.278380991834169,{"$f":"F2298*(1-Elteq!$F$5)","v":47.278380991834169}]
["ANAMET-M",8280209,"M 20 x 1,5","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",1,60.656425524795701,{"$f":"F2299*(1-Elteq!$F$5)","v":60.656425524795701}]
["ANAMET-M",8280259,"M 25 x 1,5","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",1,66.091256116311314,{"$f":"F2300*(1-Elteq!$F$5)","v":66.091256116311314}]
["ANAMET-M",8280329,"M 32 x 1,5","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",1,104.09790902210688,{"$f":"F2301*(1-Elteq!$F$5)","v":104.09790902210688}]
["ANAMET-M",8280409,"M 40 x 1,5","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",1,131.91309328022274,{"$f":"F2302*(1-Elteq!$F$5)","v":131.91309328022274}]
["ANAMET-M",2630160,"M16 x 1,5","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",1,2.5083833499302859,{"$f":"F2303*(1-Elteq!$F$5)","v":2.5083833499302859}]
["ANAMET-M",2630200,"M20 x 1,5","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",1,2.5083833499302859,{"$f":"F2304*(1-Elteq!$F$5)","v":2.5083833499302859}]
["ANAMET-M",2630250,"M25 x 1,5","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",1,3.0100600199163439,{"$f":"F2305*(1-Elteq!$F$5)","v":3.0100600199163439}]
["ANAMET-M",2630320,"M32 x 1,5","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",1,4.682315586536534,{"$f":"F2306*(1-Elteq!$F$5)","v":4.682315586536534}]
["ANAMET-M",2631160,"M16 x 1,5","Sealtite fittings for NMUA/NMSF, 90° elbow fixed with male thread, IP 67",1,2.8985763154749975,{"$f":"F2307*(1-Elteq!$F$5)","v":2.8985763154749975}]
["ANAMET-M",2631200,"M20 x 1,5","Sealtite fittings for NMUA/NMSF, 90° elbow fixed with male thread, IP 67",1,2.8985763154749975,{"$f":"F2308*(1-Elteq!$F$5)","v":2.8985763154749975}]
["ANAMET-M",2631250,"M25 x 1,5","Sealtite fittings for NMUA/NMSF, 90° elbow fixed with male thread, IP 67",1,3.3222143923521124,{"$f":"F2309*(1-Elteq!$F$5)","v":3.3222143923521124}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},2631320,"M32 x 1,5","Sealtite fittings for NMUA/NMSF, 90° elbow fixed with male thread, IP 67",1,4.8495411431985529,{"$f":"F2310*(1-Elteq!$F$5)","v":4.8495411431985529}]
["ANAMET-M",2633120,"NPT 1/2\"","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",1,2.5083833499302859,{"$f":"F2311*(1-Elteq!$F$5)","v":2.5083833499302859}]
["ANAMET-M",2633160,"NPT 1/2\"","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",1,2.5083833499302859,{"$f":"F2312*(1-Elteq!$F$5)","v":2.5083833499302859}]
["ANAMET-M",2633200,"NPT 3/4\"","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",1,3.0100600199163439,{"$f":"F2313*(1-Elteq!$F$5)","v":3.0100600199163439}]
["ANAMET-M",2633260,"NPT 1","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",1,4.682315586536534,{"$f":"F2314*(1-Elteq!$F$5)","v":4.682315586536534}]
["ANAMET-M",2633350,"NPT 1.1/4","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",1,5.5741852220673023,{"$f":"F2315*(1-Elteq!$F$5)","v":5.5741852220673023}]
["ANAMET-M",2633400,"NPT 1.1/2","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",1,7.0792152320254731,{"$f":"F2316*(1-Elteq!$F$5)","v":7.0792152320254731}]
["ANAMET-M",2633500,"NPT 2","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",1,10.535210069707201,{"$f":"F2317*(1-Elteq!$F$5)","v":10.535210069707201}]
["ANAMET-M",2634120,"NPT 1/2\"","Sealtite fittings for NMUA/NMSF, 90° elbow fixed with male thread, IP 67",1,2.8985763154749975,{"$f":"F2318*(1-Elteq!$F$5)","v":2.8985763154749975}]
["ANAMET-M",2634160,"NPT 1/2\"","Sealtite fittings for NMUA/NMSF, 90° elbow fixed with male thread, IP 67",1,2.8985763154749975,{"$f":"F2319*(1-Elteq!$F$5)","v":2.8985763154749975}]
["ANAMET-M",2634200,"NPT 3/4\"","Sealtite fittings for NMUA/NMSF, 90° elbow fixed with male thread, IP 67",1,3.3222143923521124,{"$f":"F2320*(1-Elteq!$F$5)","v":3.3222143923521124}]
["ANAMET-M",2634260,"NPT 1","Sealtite fittings for NMUA/NMSF, 90° elbow fixed with male thread, IP 67",1,4.8495411431985529,{"$f":"F2321*(1-Elteq!$F$5)","v":4.8495411431985529}]
["ANAMET-M",2634350,"NPT 1.1/4","Sealtite fittings for NMUA/NMSF, 90° elbow fixed with male thread, IP 67",1,8.5842452419836466,{"$f":"F2322*(1-Elteq!$F$5)","v":8.5842452419836466}]
["ANAMET-M",2634400,"NPT 1.1/2","Sealtite fittings for NMUA/NMSF, 90° elbow fixed with male thread, IP 67",1,11.129789826727714,{"$f":"F2323*(1-Elteq!$F$5)","v":11.129789826727714}]
["ANAMET-M",2634500,"NPT 2","Sealtite fittings for NMUA/NMSF, 90° elbow fixed with male thread, IP 67",1,16.889781222863927,{"$f":"F2324*(1-Elteq!$F$5)","v":16.889781222863927}]
["ANAMET-M",8100101,"PG 9","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,4.756638056164098,{"$f":"F2325*(1-Elteq!$F$5)","v":4.756638056164098}]
["ANAMET-M",8100111,"PG 11","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,4.8867023780123349,{"$f":"F2326*(1-Elteq!$F$5)","v":4.8867023780123349}]
["ANAMET-M",8100131,"PG 13,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,4.8867023780123349,{"$f":"F2327*(1-Elteq!$F$5)","v":4.8867023780123349}]
["ANAMET-M",8100161,"PG 16","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,5.7042495439155392,{"$f":"F2328*(1-Elteq!$F$5)","v":5.7042495439155392}]
["ANAMET-M",8100210,"M25 x 1,5","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",1,12.17030440151361,{"$f":"F2329*(1-Elteq!$F$5)","v":12.17030440151361}]
["ANAMET-M",8100211,"PG 21","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,7.5530209759011955,{"$f":"F2330*(1-Elteq!$F$5)","v":7.5530209759011955}]
["ANAMET-M",8100291,"PG 29","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,13.006432184823705,{"$f":"F2331*(1-Elteq!$F$5)","v":13.006432184823705}]
["ANAMET-M",8100361,"PG 36","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,21.414161561441887,{"$f":"F2332*(1-Elteq!$F$5)","v":21.414161561441887}]
["ANAMET-M",8100421,"PG 42","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,28.734924819756944,{"$f":"F2333*(1-Elteq!$F$5)","v":28.734924819756944}]
["ANAMET-M",8100481,"PG 48","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,44.063934180442025,{"$f":"F2334*(1-Elteq!$F$5)","v":44.063934180442025}]
["ANAMET-M",8120161,"M16 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,4.5801221907986331,{"$f":"F2335*(1-Elteq!$F$5)","v":4.5801221907986331}]
["ANAMET-M",8120171,"M20 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,4.9238636128261177,{"$f":"F2336*(1-Elteq!$F$5)","v":4.9238636128261177}]
["ANAMET-M",8120201,"M20 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,4.9238636128261177,{"$f":"F2337*(1-Elteq!$F$5)","v":4.9238636128261177}]
["ANAMET-M",8120250,"M25 x 1,5","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",1,7.6087628281218675,{"$f":"F2338*(1-Elteq!$F$5)","v":7.6087628281218675}]
["ANAMET-M",8120321,"M32 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,11.61288587930688,{"$f":"F2339*(1-Elteq!$F$5)","v":11.61288587930688}]
["ANAMET-M",8120401,"M40 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,21.414161561441887,{"$f":"F2340*(1-Elteq!$F$5)","v":21.414161561441887}]
["ANAMET-M",8120501,"M50 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,28.734924819756944,{"$f":"F2341*(1-Elteq!$F$5)","v":28.734924819756944}]
["ANAMET-M",8120631,"M63 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,44.063934180442025,{"$f":"F2342*(1-Elteq!$F$5)","v":44.063934180442025}]
["ANAMET-M",8189161,"M16 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",1,16.165137143995175,{"$f":"F2343*(1-Elteq!$F$5)","v":16.165137143995175}]
["ANAMET-M",8189201,"M20 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",1,20.624485321649018,{"$f":"F2344*(1-Elteq!$F$5)","v":20.624485321649018}]
["ANAMET-M",8189251,"M25 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",1,26.087186839274974,{"$f":"F2345*(1-Elteq!$F$5)","v":26.087186839274974}]
["ANAMET-M",8189321,"M32 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",1,45.485351412069186,{"$f":"F2346*(1-Elteq!$F$5)","v":45.485351412069186}]
["ANAMET-M",8320169,"M 16 x 1,5","Food grade fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,49.136442732523271,{"$f":"F2347*(1-Elteq!$F$5)","v":49.136442732523271}]
["ANAMET-M",8320209,"M 20 x 1,5","Food grade fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,49.136442732523271,{"$f":"F2348*(1-Elteq!$F$5)","v":49.136442732523271}]
["ANAMET-M",8320259,"M 25 x 1,5","Food grade fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,66.481449081856027,{"$f":"F2349*(1-Elteq!$F$5)","v":66.481449081856027}]
["ANAMET-M",8320329,"M 32 x 1,5","Food grade fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,98.337917625970647,{"$f":"F2350*(1-Elteq!$F$5)","v":98.337917625970647}]
["ANAMET-M",6505092,"ADU-K","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",1,3.0843824895439074,{"$f":"F2351*(1-Elteq!$F$5)","v":3.0843824895439074}]
["ANAMET-M",6505112,"ADU-K","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",1,3.9483811989643396,{"$f":"F2352*(1-Elteq!$F$5)","v":3.9483811989643396}]
["ANAMET-M",6505132,"ADU-K","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",1,4.8123799083847709,{"$f":"F2353*(1-Elteq!$F$5)","v":4.8123799083847709}]
["ANAMET-M",6505162,"ADU-K","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",1,6.1316037442740328,{"$f":"F2354*(1-Elteq!$F$5)","v":6.1316037442740328}]
["ANAMET-M",6505212,"ADU-K","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",1,7.2185698625771559,{"$f":"F2355*(1-Elteq!$F$5)","v":7.2185698625771559}]
["ANAMET-M",6505292,"ADU-K","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",1,12.922819406492696,{"$f":"F2356*(1-Elteq!$F$5)","v":12.922819406492696}]
["ANAMET-M",6505362,"ADU-K","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",1,18.840746050587484,{"$f":"F2357*(1-Elteq!$F$5)","v":18.840746050587484}]
["ANAMET-M",6505422,"ADU-K","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",1,20.104228034256071,{"$f":"F2358*(1-Elteq!$F$5)","v":20.104228034256071}]
["ANAMET-M",6505482,"ADU-K","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",1,22.352482740489879,{"$f":"F2359*(1-Elteq!$F$5)","v":22.352482740489879}]
["ANAMET-M",6506093,"ADU-H","Sealtite fittings for MPC/MPU, Straight swivel box connector, IP 54",1,6.1316037442740328,{"$f":"F2360*(1-Elteq!$F$5)","v":6.1316037442740328}]
["ANAMET-M",6506113,"ADU-H","Sealtite fittings for MPC/MPU, Straight swivel box connector, IP 54",1,6.3452808444532796,{"$f":"F2361*(1-Elteq!$F$5)","v":6.3452808444532796}]
["ANAMET-M",6506133,"ADU-H","Sealtite fittings for MPC/MPU, Straight swivel box connector, IP 54",1,6.5589579446325255,{"$f":"F2362*(1-Elteq!$F$5)","v":6.5589579446325255}]
["ANAMET-M",6506163,"ADU-H","Sealtite fittings for MPC/MPU, Straight swivel box connector, IP 54",1,6.7912156622186624,{"$f":"F2363*(1-Elteq!$F$5)","v":6.7912156622186624}]
["ANAMET-M",6506213,"ADU-H","Sealtite fittings for MPC/MPU, Straight swivel box connector, IP 54",1,7.4508275801632937,{"$f":"F2364*(1-Elteq!$F$5)","v":7.4508275801632937}]
["ANAMET-M",6506293,"ADU-H","Sealtite fittings for MPC/MPU, Straight swivel box connector, IP 54",1,8.110439498107926,{"$f":"F2365*(1-Elteq!$F$5)","v":8.110439498107926}]
["ANAMET-M",6507092,"AUK-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,8.6306967855008718,{"$f":"F2366*(1-Elteq!$F$5)","v":8.6306967855008718}]
["ANAMET-M",6507112,"AUK-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,8.6306967855008718,{"$f":"F2367*(1-Elteq!$F$5)","v":8.6306967855008718}]
["ANAMET-M",6507132,"AUK-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,9.0394703684524753,{"$f":"F2368*(1-Elteq!$F$5)","v":9.0394703684524753}]
["ANAMET-M",6507162,"AUK-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,12.421142736506638,{"$f":"F2369*(1-Elteq!$F$5)","v":12.421142736506638}]
["ANAMET-M",6507212,"AUK-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,14.753010221071461,{"$f":"F2370*(1-Elteq!$F$5)","v":14.753010221071461}]
["ANAMET-M",6507292,"AUK-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,19.955583095000943,{"$f":"F2371*(1-Elteq!$F$5)","v":19.955583095000943}]
["ANAMET-M",6507362,"AUK-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,32.553241696873044,{"$f":"F2372*(1-Elteq!$F$5)","v":32.553241696873044}]
["ANAMET-M",6507422,"AUK-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,55.909077777335042,{"$f":"F2373*(1-Elteq!$F$5)","v":55.909077777335042}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},6507482,"AUK-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,55.909077777335042,{"$f":"F2374*(1-Elteq!$F$5)","v":55.909077777335042}]
["ANAMET-M",6508094,"AUM-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,9.3739214817765131,{"$f":"F2375*(1-Elteq!$F$5)","v":9.3739214817765131}]
["ANAMET-M",6508114,"AUM-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,12.523336132244539,{"$f":"F2376*(1-Elteq!$F$5)","v":12.523336132244539}]
["ANAMET-M",6508134,"AUM-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,12.523336132244539,{"$f":"F2377*(1-Elteq!$F$5)","v":12.523336132244539}]
["ANAMET-M",6508164,"AUM-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,13.851850276837247,{"$f":"F2378*(1-Elteq!$F$5)","v":13.851850276837247}]
["ANAMET-M",6508214,"AUM-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,19.853389699263044,{"$f":"F2379*(1-Elteq!$F$5)","v":19.853389699263044}]
["ANAMET-M",6508294,"AUM-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,30.249245138418562,{"$f":"F2380*(1-Elteq!$F$5)","v":30.249245138418562}]
["ANAMET-M",6508364,"AUM-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,50.892311077474474,{"$f":"F2381*(1-Elteq!$F$5)","v":50.892311077474474}]
["ANAMET-M",6508424,"AUM-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,81.912651838279004,{"$f":"F2382*(1-Elteq!$F$5)","v":81.912651838279004}]
["ANAMET-M",6508484,"AUM-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,83.510584935271638,{"$f":"F2383*(1-Elteq!$F$5)","v":83.510584935271638}]
["ANAMET-M",6513162,"ADU-KM","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",1,3.0843824895439074,{"$f":"F2384*(1-Elteq!$F$5)","v":3.0843824895439074}]
["ANAMET-M",6513202,"ADU-KM","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",1,3.9483811989643396,{"$f":"F2385*(1-Elteq!$F$5)","v":3.9483811989643396}]
["ANAMET-M",6513252,"ADU-KM","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",1,6.1316037442740328,{"$f":"F2386*(1-Elteq!$F$5)","v":6.1316037442740328}]
["ANAMET-M",6513322,"ADU-KM","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",1,7.2185698625771559,{"$f":"F2387*(1-Elteq!$F$5)","v":7.2185698625771559}]
["ANAMET-M",6513402,"ADU-KM","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",1,12.922819406492696,{"$f":"F2388*(1-Elteq!$F$5)","v":12.922819406492696}]
["ANAMET-M",6513502,"ADU-KM","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",1,18.840746050587484,{"$f":"F2389*(1-Elteq!$F$5)","v":18.840746050587484}]
["ANAMET-M",6513632,"ADU-KM","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",1,22.352482740489879,{"$f":"F2390*(1-Elteq!$F$5)","v":22.352482740489879}]
["ANAMET-M",6517162,"AUK-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,7.1814086277633749,{"$f":"F2391*(1-Elteq!$F$5)","v":7.1814086277633749}]
["ANAMET-M",6517172,"AUK-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,8.3241165982871728,{"$f":"F2392*(1-Elteq!$F$5)","v":8.3241165982871728}]
["ANAMET-M",6517202,"AUK-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,12.328239649472183,{"$f":"F2393*(1-Elteq!$F$5)","v":12.328239649472183}]
["ANAMET-M",6517252,"AUK-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,14.418559107747422,{"$f":"F2394*(1-Elteq!$F$5)","v":14.418559107747422}]
["ANAMET-M",6517322,"AUK-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,19.751196303525145,{"$f":"F2395*(1-Elteq!$F$5)","v":19.751196303525145}]
["ANAMET-M",6517402,"AUK-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,31.178276008763117,{"$f":"F2396*(1-Elteq!$F$5)","v":31.178276008763117}]
["ANAMET-M",6517502,"AUK-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,53.781597084246023,{"$f":"F2397*(1-Elteq!$F$5)","v":53.781597084246023}]
["ANAMET-M",6517632,"AUK-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,55.909077777335042,{"$f":"F2398*(1-Elteq!$F$5)","v":55.909077777335042}]
["ANAMET-M",6518124,"AUP-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,9.8477272256522355,{"$f":"F2399*(1-Elteq!$F$5)","v":9.8477272256522355}]
["ANAMET-M",6518164,"AUP-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,13.155077124078835,{"$f":"F2400*(1-Elteq!$F$5)","v":13.155077124078835}]
["ANAMET-M",6518174,"AUP-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,13.155077124078835,{"$f":"F2401*(1-Elteq!$F$5)","v":13.155077124078835}]
["ANAMET-M",6518204,"AUP-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,14.54862342959566,{"$f":"F2402*(1-Elteq!$F$5)","v":14.54862342959566}]
["ANAMET-M",6518254,"AUP-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,18.692101111332356,{"$f":"F2403*(1-Elteq!$F$5)","v":18.692101111332356}]
["ANAMET-M",6518324,"AUP-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,31.772855765783625,{"$f":"F2404*(1-Elteq!$F$5)","v":31.772855765783625}]
["ANAMET-M",6518404,"AUP-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,53.437855662218546,{"$f":"F2405*(1-Elteq!$F$5)","v":53.437855662218546}]
["ANAMET-M",6518504,"AUP-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,86.009677976498466,{"$f":"F2406*(1-Elteq!$F$5)","v":86.009677976498466}]
["ANAMET-M",6518634,"AUP-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",1,87.691223851822116,{"$f":"F2407*(1-Elteq!$F$5)","v":87.691223851822116}]
["ANAMET-M",2670160,"SVCHF M16 B-12","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",1,7.3950857279426208,{"$f":"F2408*(1-Elteq!$F$5)","v":7.3950857279426208}]
["ANAMET-M",2670161,"SVCHF M16 B-10","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",1,7.2650214060943847,{"$f":"F2409*(1-Elteq!$F$5)","v":7.2650214060943847}]
["ANAMET-M",2670200,"SVCHF M20 B-17","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",1,8.7979223421628934,{"$f":"F2410*(1-Elteq!$F$5)","v":8.7979223421628934}]
["ANAMET-M",2670201,"SVCHF M20 B-12","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",1,8.3891487592112899,{"$f":"F2411*(1-Elteq!$F$5)","v":8.3891487592112899}]
["ANAMET-M",2670202,"SVCHF M20 B-23","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",1,9.1045025293765942,{"$f":"F2412*(1-Elteq!$F$5)","v":9.1045025293765942}]
["ANAMET-M",2670250,"SVCHF M25 B-23","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",1,15.533396152160881,{"$f":"F2413*(1-Elteq!$F$5)","v":15.533396152160881}]
["ANAMET-M",2670251,"SVCHF M25 B-17","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",1,9.5132761123281959,{"$f":"F2414*(1-Elteq!$F$5)","v":9.5132761123281959}]
["ANAMET-M",2670320,"SVCHF M32 B-29","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",1,16.611071961760562,{"$f":"F2415*(1-Elteq!$F$5)","v":16.611071961760562}]
["ANAMET-M",2680120,"SV M12 G-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.6536749492132996,{"$f":"F2416*(1-Elteq!$F$5)","v":1.6536749492132996}]
["ANAMET-M",2680121,"SV M12 G-7,5","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.5886427882891812,{"$f":"F2417*(1-Elteq!$F$5)","v":1.5886427882891812}]
["ANAMET-M",2680160,"SV M16 G-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.9138035929097739,{"$f":"F2418*(1-Elteq!$F$5)","v":1.9138035929097739}]
["ANAMET-M",2680161,"SV M16 G-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.7930295797649822,{"$f":"F2419*(1-Elteq!$F$5)","v":1.7930295797649822}]
["ANAMET-M",2680200,"SV M20 G-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.8580617406891009,{"$f":"F2420*(1-Elteq!$F$5)","v":1.8580617406891009}]
["ANAMET-M",2680201,"SV M20 G-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.8580617406891009,{"$f":"F2421*(1-Elteq!$F$5)","v":1.8580617406891009}]
["ANAMET-M",2680250,"SV M25 G-23","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,3.7904459510057658,{"$f":"F2422*(1-Elteq!$F$5)","v":3.7904459510057658}]
["ANAMET-M",2680251,"SV M25 G-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,2.2575450149372576,{"$f":"F2423*(1-Elteq!$F$5)","v":2.2575450149372576}]
["ANAMET-M",2680320,"SV M32 G-29","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,4.7101865126468709,{"$f":"F2424*(1-Elteq!$F$5)","v":4.7101865126468709}]
["ANAMET-M",2680400,"SV M40 G-37","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,6.4381839314877336,{"$f":"F2425*(1-Elteq!$F$5)","v":6.4381839314877336}]
["ANAMET-M",2680500,"SV M50 G-48","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,7.7574077673769963,{"$f":"F2426*(1-Elteq!$F$5)","v":7.7574077673769963}]
["ANAMET-M",2680630,"SV M63 G-48","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,8.3984390679147349,{"$f":"F2427*(1-Elteq!$F$5)","v":8.3984390679147349}]
["ANAMET-M",2681120,"SV M12 B-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.6536749492132996,{"$f":"F2428*(1-Elteq!$F$5)","v":1.6536749492132996}]
["ANAMET-M",2681121,"SV M12 B-7,5","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.5886427882891812,{"$f":"F2429*(1-Elteq!$F$5)","v":1.5886427882891812}]
["ANAMET-M",2681160,"SV M16 B-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.9138035929097739,{"$f":"F2430*(1-Elteq!$F$5)","v":1.9138035929097739}]
["ANAMET-M",2681161,"SV M16 B-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.7930295797649822,{"$f":"F2431*(1-Elteq!$F$5)","v":1.7930295797649822}]
["ANAMET-M",2681200,"SV M20 B-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.8580617406891009,{"$f":"F2432*(1-Elteq!$F$5)","v":1.8580617406891009}]
["ANAMET-M",2681201,"SV M20 B-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.8580617406891009,{"$f":"F2433*(1-Elteq!$F$5)","v":1.8580617406891009}]
["ANAMET-M",2681250,"SV M25 B-23","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,3.7904459510057658,{"$f":"F2434*(1-Elteq!$F$5)","v":3.7904459510057658}]
["ANAMET-M",2681251,"SV M25 B-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,2.2575450149372576,{"$f":"F2435*(1-Elteq!$F$5)","v":2.2575450149372576}]
["ANAMET-M",2681320,"SV M32 B-29","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,4.7101865126468709,{"$f":"F2436*(1-Elteq!$F$5)","v":4.7101865126468709}]
["ANAMET-M",2681400,"SV M40 B-37","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,6.4381839314877336,{"$f":"F2437*(1-Elteq!$F$5)","v":6.4381839314877336}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},2681500,"SV M50 B-48","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,7.7574077673769963,{"$f":"F2438*(1-Elteq!$F$5)","v":7.7574077673769963}]
["ANAMET-M",2681630,"SV M63 B-48","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,8.3984390679147349,{"$f":"F2439*(1-Elteq!$F$5)","v":8.3984390679147349}]
["ANAMET-M",2683160,"SV 90 M16 B-12","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,3.6603816291575288,{"$f":"F2440*(1-Elteq!$F$5)","v":3.6603816291575288}]
["ANAMET-M",2683161,"SV 90 M16 B-10","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,3.4931560724955091,{"$f":"F2441*(1-Elteq!$F$5)","v":3.4931560724955091}]
["ANAMET-M",2683200,"SV 90 M20 B-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,4.3199935471021602,{"$f":"F2442*(1-Elteq!$F$5)","v":4.3199935471021602}]
["ANAMET-M",2683201,"SV 90 M20 B-12","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,3.9576715076677846,{"$f":"F2443*(1-Elteq!$F$5)","v":3.9576715076677846}]
["ANAMET-M",2683250,"SV 90 M25 B-23","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,6.0851522007568049,{"$f":"F2444*(1-Elteq!$F$5)","v":6.0851522007568049}]
["ANAMET-M",2683251,"SV 90 M25 B-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,4.5522512646882971,{"$f":"F2445*(1-Elteq!$F$5)","v":4.5522512646882971}]
["ANAMET-M",2683320,"SV 90 M32 B-29","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,9.40179240788685,{"$f":"F2446*(1-Elteq!$F$5)","v":9.40179240788685}]
["ANAMET-M",2683321,"SV 90 M32 B-23","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,7.4508275801632937,{"$f":"F2447*(1-Elteq!$F$5)","v":7.4508275801632937}]
["ANAMET-M",2683400,"SV 90 M40 B-36","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,15.189654730133402,{"$f":"F2448*(1-Elteq!$F$5)","v":15.189654730133402}]
["ANAMET-M",2683401,"SV 90 M40 B-29","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,10.58166161322443,{"$f":"F2449*(1-Elteq!$F$5)","v":10.58166161322443}]
["ANAMET-M",2683500,"SV 90 M50 B-48","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,18.088231045608396,{"$f":"F2450*(1-Elteq!$F$5)","v":18.088231045608396}]
["ANAMET-M",2683501,"SV 90 M50 B-36","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,15.728492634933239,{"$f":"F2451*(1-Elteq!$F$5)","v":15.728492634933239}]
["ANAMET-M",2683630,"SV 90 M63 B-48","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,18.859326667994374,{"$f":"F2452*(1-Elteq!$F$5)","v":18.859326667994374}]
["ANAMET-M",2671090,"SVCHF PG 9 B-10","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",1,7.6923756064528774,{"$f":"F2453*(1-Elteq!$F$5)","v":7.6923756064528774}]
["ANAMET-M",2671110,"SVCHF PG11 B-12","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",1,7.8038593108942234,{"$f":"F2454*(1-Elteq!$F$5)","v":7.8038593108942234}]
["ANAMET-M",2671130,"SVCHF PG 13,5 B-17","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",1,9.2159862338179401,{"$f":"F2455*(1-Elteq!$F$5)","v":9.2159862338179401}]
["ANAMET-M",2671131,"SVCHF PG 13,5 B-12","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",1,8.7979223421628934,{"$f":"F2456*(1-Elteq!$F$5)","v":8.7979223421628934}]
["ANAMET-M",2671160,"SVCHF PG 16 B-17","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",1,9.5132761123281959,{"$f":"F2457*(1-Elteq!$F$5)","v":9.5132761123281959}]
["ANAMET-M",2671210,"SVCHF PG 21 B-23","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",1,16.313782083250302,{"$f":"F2458*(1-Elteq!$F$5)","v":16.313782083250302}]
["ANAMET-M",2671290,"SVCHF PG 29 B-29","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",1,17.428619127663769,{"$f":"F2459*(1-Elteq!$F$5)","v":17.428619127663769}]
["ANAMET-M",2682160,"SV 90 M16 G-12","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,3.6603816291575288,{"$f":"F2460*(1-Elteq!$F$5)","v":3.6603816291575288}]
["ANAMET-M",2682161,"SV 90 M16 G-10","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,3.4931560724955091,{"$f":"F2461*(1-Elteq!$F$5)","v":3.4931560724955091}]
["ANAMET-M",2682200,"SV 90 M20 G-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,4.3199935471021602,{"$f":"F2462*(1-Elteq!$F$5)","v":4.3199935471021602}]
["ANAMET-M",2682201,"SV 90 M20 G-12","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,3.9576715076677846,{"$f":"F2463*(1-Elteq!$F$5)","v":3.9576715076677846}]
["ANAMET-M",2682250,"SV 90 M25 G-23","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,6.0851522007568049,{"$f":"F2464*(1-Elteq!$F$5)","v":6.0851522007568049}]
["ANAMET-M",2682251,"SV 90 M25 G-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,4.5522512646882971,{"$f":"F2465*(1-Elteq!$F$5)","v":4.5522512646882971}]
["ANAMET-M",2682320,"SV 90 M32 G-29","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,9.40179240788685,{"$f":"F2466*(1-Elteq!$F$5)","v":9.40179240788685}]
["ANAMET-M",2682321,"SV 90 M32 G-23","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,7.4508275801632937,{"$f":"F2467*(1-Elteq!$F$5)","v":7.4508275801632937}]
["ANAMET-M",2682400,"SV 90 M40 G-36","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,15.189654730133402,{"$f":"F2468*(1-Elteq!$F$5)","v":15.189654730133402}]
["ANAMET-M",2682401,"SV 90 M40 G-29","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,10.58166161322443,{"$f":"F2469*(1-Elteq!$F$5)","v":10.58166161322443}]
["ANAMET-M",2682500,"SV 90 M50 G-48","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,18.088231045608396,{"$f":"F2470*(1-Elteq!$F$5)","v":18.088231045608396}]
["ANAMET-M",2682501,"SV 90 M50 G-36","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,15.728492634933239,{"$f":"F2471*(1-Elteq!$F$5)","v":15.728492634933239}]
["ANAMET-M",2682630,"SV 90 M63 G-48","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,18.859326667994374,{"$f":"F2472*(1-Elteq!$F$5)","v":18.859326667994374}]
["ANAMET-M",2684070,"SV PG 7 G-7,5","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.5886427882891812,{"$f":"F2473*(1-Elteq!$F$5)","v":1.5886427882891812}]
["ANAMET-M",2684071,"SV PG 7 G-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.6536749492132996,{"$f":"F2474*(1-Elteq!$F$5)","v":1.6536749492132996}]
["ANAMET-M",2684090,"SV PG 9 G-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.6536749492132996,{"$f":"F2475*(1-Elteq!$F$5)","v":1.6536749492132996}]
["ANAMET-M",2684091,"SV PG 9 G-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.8301908145787644,{"$f":"F2476*(1-Elteq!$F$5)","v":1.8301908145787644}]
["ANAMET-M",2684110,"SV PG 11 G-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.8301908145787644,{"$f":"F2477*(1-Elteq!$F$5)","v":1.8301908145787644}]
["ANAMET-M",2684111,"SV PG 11 G-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.9602551364270013,{"$f":"F2478*(1-Elteq!$F$5)","v":1.9602551364270013}]
["ANAMET-M",2684130,"SV PG 13 G-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,2.0438679147580112,{"$f":"F2479*(1-Elteq!$F$5)","v":2.0438679147580112}]
["ANAMET-M",2684131,"SV PG 13 G-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,2.0438679147580112,{"$f":"F2480*(1-Elteq!$F$5)","v":2.0438679147580112}]
["ANAMET-M",2684160,"SV PG 16 G-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,2.1367710017924657,{"$f":"F2481*(1-Elteq!$F$5)","v":2.1367710017924657}]
["ANAMET-M",2684210,"SV PG 21 G-23","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,4.5429609559848512,{"$f":"F2482*(1-Elteq!$F$5)","v":4.5429609559848512}]
["ANAMET-M",2684290,"SV PG 29 G-29","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,4.9424442302330078,{"$f":"F2483*(1-Elteq!$F$5)","v":4.9424442302330078}]
["ANAMET-M",2684360,"SV PG 36 G-36","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,6.4381839314877336,{"$f":"F2484*(1-Elteq!$F$5)","v":6.4381839314877336}]
["ANAMET-M",2684480,"SV PG 48 G-48","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,8.5006324636526376,{"$f":"F2485*(1-Elteq!$F$5)","v":8.5006324636526376}]
["ANAMET-M",2685070,"SV PG 7 B-7,5","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.5886427882891812,{"$f":"F2486*(1-Elteq!$F$5)","v":1.5886427882891812}]
["ANAMET-M",2685071,"SV PG 7 B-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.6536749492132996,{"$f":"F2487*(1-Elteq!$F$5)","v":1.6536749492132996}]
["ANAMET-M",2685090,"SV PG 9 B-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.6536749492132996,{"$f":"F2488*(1-Elteq!$F$5)","v":1.6536749492132996}]
["ANAMET-M",2685091,"SV PG 9 B-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.8301908145787644,{"$f":"F2489*(1-Elteq!$F$5)","v":1.8301908145787644}]
["ANAMET-M",2685110,"SV PG 11 B-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.8301908145787644,{"$f":"F2490*(1-Elteq!$F$5)","v":1.8301908145787644}]
["ANAMET-M",2685111,"SV PG 11 B-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,1.9602551364270013,{"$f":"F2491*(1-Elteq!$F$5)","v":1.9602551364270013}]
["ANAMET-M",2685130,"SV PG 13 B-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,2.0438679147580112,{"$f":"F2492*(1-Elteq!$F$5)","v":2.0438679147580112}]
["ANAMET-M",2685131,"SV PG 13 B-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,2.0438679147580112,{"$f":"F2493*(1-Elteq!$F$5)","v":2.0438679147580112}]
["ANAMET-M",2685160,"SV PG 16 B-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,2.1367710017924657,{"$f":"F2494*(1-Elteq!$F$5)","v":2.1367710017924657}]
["ANAMET-M",2685210,"SV PG 21 B-23","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,4.5429609559848512,{"$f":"F2495*(1-Elteq!$F$5)","v":4.5429609559848512}]
["ANAMET-M",2685290,"SV PG 29 B-29","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,4.9424442302330078,{"$f":"F2496*(1-Elteq!$F$5)","v":4.9424442302330078}]
["ANAMET-M",2685360,"SV PG 36 B-36","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,6.4381839314877336,{"$f":"F2497*(1-Elteq!$F$5)","v":6.4381839314877336}]
["ANAMET-M",2685480,"SV PG 48 B-48","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,8.5006324636526376,{"$f":"F2498*(1-Elteq!$F$5)","v":8.5006324636526376}]
["ANAMET-M",2686090,"SV 90 PG 9 G-10","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,3.4931560724955091,{"$f":"F2499*(1-Elteq!$F$5)","v":3.4931560724955091}]
["ANAMET-M",2686110,"SV 90 PG 11 G-12","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,3.8461878032264387,{"$f":"F2500*(1-Elteq!$F$5)","v":3.8461878032264387}]
["ANAMET-M",2686130,"SV 90 PG 13 G-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,4.0784455208125756,{"$f":"F2501*(1-Elteq!$F$5)","v":4.0784455208125756}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},2686160,"SV 90 PG 16 G-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,4.2549613861780404,{"$f":"F2502*(1-Elteq!$F$5)","v":4.2549613861780404}]
["ANAMET-M",2686210,"SV 90 PG 21 G-23","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,6.0851522007568049,{"$f":"F2503*(1-Elteq!$F$5)","v":6.0851522007568049}]
["ANAMET-M",2686290,"SV 90 PG 29 G-29","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,9.40179240788685,{"$f":"F2504*(1-Elteq!$F$5)","v":9.40179240788685}]
["ANAMET-M",2686360,"SV 90 PG 36 G-36","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,15.189654730133402,{"$f":"F2505*(1-Elteq!$F$5)","v":15.189654730133402}]
["ANAMET-M",2686480,"SV 90 PG 48 G-48","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,18.794294507070255,{"$f":"F2506*(1-Elteq!$F$5)","v":18.794294507070255}]
["ANAMET-M",2687090,"SV 90 PG 9 B-10","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,3.4931560724955091,{"$f":"F2507*(1-Elteq!$F$5)","v":3.4931560724955091}]
["ANAMET-M",2687110,"SV 90 PG 11 B-12","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,3.8461878032264387,{"$f":"F2508*(1-Elteq!$F$5)","v":3.8461878032264387}]
["ANAMET-M",2687130,"SV 90 PG 13 B-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,4.0784455208125756,{"$f":"F2509*(1-Elteq!$F$5)","v":4.0784455208125756}]
["ANAMET-M",2687160,"SV 90 PG 16 B-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,4.2549613861780404,{"$f":"F2510*(1-Elteq!$F$5)","v":4.2549613861780404}]
["ANAMET-M",2687210,"SV 90 PG 21 B-23","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,6.0851522007568049,{"$f":"F2511*(1-Elteq!$F$5)","v":6.0851522007568049}]
["ANAMET-M",2687290,"SV 90 PG 29 B-29","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,9.40179240788685,{"$f":"F2512*(1-Elteq!$F$5)","v":9.40179240788685}]
["ANAMET-M",2687360,"SV 90 PG 36 B-36","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,15.189654730133402,{"$f":"F2513*(1-Elteq!$F$5)","v":15.189654730133402}]
["ANAMET-M",2687480,"SV 90 PG 48 B-48","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,18.794294507070255,{"$f":"F2514*(1-Elteq!$F$5)","v":18.794294507070255}]
["ANAMET-M",2688070,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",1,0.11148370444134605,{"$f":"F2515*(1-Elteq!$F$5)","v":0.11148370444134605}]
["ANAMET-M",2688100,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",1,0.11148370444134605,{"$f":"F2516*(1-Elteq!$F$5)","v":0.11148370444134605}]
["ANAMET-M",2688120,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",1,0.11148370444134605,{"$f":"F2517*(1-Elteq!$F$5)","v":0.11148370444134605}]
["ANAMET-M",2688130,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",1,0.11148370444134605,{"$f":"F2518*(1-Elteq!$F$5)","v":0.11148370444134605}]
["ANAMET-M",2688170,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",1,0.16722555666201905,{"$f":"F2519*(1-Elteq!$F$5)","v":0.16722555666201905}]
["ANAMET-M",2688180,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",1,0.16722555666201905,{"$f":"F2520*(1-Elteq!$F$5)","v":0.16722555666201905}]
["ANAMET-M",2688230,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",1,0.16722555666201905,{"$f":"F2521*(1-Elteq!$F$5)","v":0.16722555666201905}]
["ANAMET-M",2688290,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",1,0.22296740888269209,{"$f":"F2522*(1-Elteq!$F$5)","v":0.22296740888269209}]
["ANAMET-M",2688300,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",1,0.22296740888269209,{"$f":"F2523*(1-Elteq!$F$5)","v":0.22296740888269209}]
["ANAMET-M",2688370,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",1,0.22296740888269209,{"$f":"F2524*(1-Elteq!$F$5)","v":0.22296740888269209}]
["ANAMET-M",2688400,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",1,0.27870926110336514,{"$f":"F2525*(1-Elteq!$F$5)","v":0.27870926110336514}]
["ANAMET-M",2688500,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",1,0.27870926110336514,{"$f":"F2526*(1-Elteq!$F$5)","v":0.27870926110336514}]
["ANAMET-M",2651160,"MSV M16 B-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,14.019075833499265,{"$f":"F2527*(1-Elteq!$F$5)","v":14.019075833499265}]
["ANAMET-M",2651161,"MSV M16 B-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,13.006432184823705,{"$f":"F2528*(1-Elteq!$F$5)","v":13.006432184823705}]
["ANAMET-M",2651200,"MSV M20 B-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,16.42526578769165,{"$f":"F2529*(1-Elteq!$F$5)","v":16.42526578769165}]
["ANAMET-M",2651201,"MSV M20 B-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,15.022429173471382,{"$f":"F2530*(1-Elteq!$F$5)","v":15.022429173471382}]
["ANAMET-M",2651250,"MSV M25 B-23","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,23.430158550089562,{"$f":"F2531*(1-Elteq!$F$5)","v":23.430158550089562}]
["ANAMET-M",2651251,"MSV M25 B-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,17.512231905994774,{"$f":"F2532*(1-Elteq!$F$5)","v":17.512231905994774}]
["ANAMET-M",2651320,"MSV M32 B-29","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,29.450278589922249,{"$f":"F2533*(1-Elteq!$F$5)","v":29.450278589922249}]
["ANAMET-M",2651400,"MSV M40 B-37","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,48.774120693088896,{"$f":"F2534*(1-Elteq!$F$5)","v":48.774120693088896}]
["ANAMET-M",2651500,"MSV M50 B-48","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,56.893850499900267,{"$f":"F2535*(1-Elteq!$F$5)","v":56.893850499900267}]
["ANAMET-M",2651630,"MSV M63 B-48","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,70.104669476199774,{"$f":"F2536*(1-Elteq!$F$5)","v":70.104669476199774}]
["ANAMET-M",2653160,"MSV 90 M16 B-12","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,16.824749061939809,{"$f":"F2537*(1-Elteq!$F$5)","v":16.824749061939809}]
["ANAMET-M",2653161,"MSV 90 M16 B-10","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,16.824749061939809,{"$f":"F2538*(1-Elteq!$F$5)","v":16.824749061939809}]
["ANAMET-M",2653200,"MSV 90 M20 B-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,18.524875554670338,{"$f":"F2539*(1-Elteq!$F$5)","v":18.524875554670338}]
["ANAMET-M",2653201,"MSV 90 M20 B-12","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,16.824749061939809,{"$f":"F2540*(1-Elteq!$F$5)","v":16.824749061939809}]
["ANAMET-M",2653250,"MSV 90 M25 B-23","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,19.723325377414806,{"$f":"F2541*(1-Elteq!$F$5)","v":19.723325377414806}]
["ANAMET-M",2653251,"MSV 90 M25 B-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,26.728218139812714,{"$f":"F2542*(1-Elteq!$F$5)","v":26.728218139812714}]
["ANAMET-M",2653320,"MSV 90 M32 B-29","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,30.044858346942764,{"$f":"F2543*(1-Elteq!$F$5)","v":30.044858346942764}]
["ANAMET-M",2653400,"MSV 90 M40 B-36","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,54.692047337183681,{"$f":"F2544*(1-Elteq!$F$5)","v":54.692047337183681}]
["ANAMET-M",2653501,"MSV 90 M50 B-36","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,56.661592782314131,{"$f":"F2545*(1-Elteq!$F$5)","v":56.661592782314131}]
["ANAMET-M",2653630,"MSV 90 M63 B-48","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,86.241935694084617,{"$f":"F2546*(1-Elteq!$F$5)","v":86.241935694084617}]
["ANAMET-M",2655090,"MSV PG 9 B-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,13.006432184823705,{"$f":"F2547*(1-Elteq!$F$5)","v":13.006432184823705}]
["ANAMET-M",2655110,"MSV PG 11 B-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,15.022429173471382,{"$f":"F2548*(1-Elteq!$F$5)","v":15.022429173471382}]
["ANAMET-M",2655131,"MSV PG 13 B-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,16.42526578769165,{"$f":"F2549*(1-Elteq!$F$5)","v":16.42526578769165}]
["ANAMET-M",2655160,"MSV PG 16 B-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,17.512231905994774,{"$f":"F2550*(1-Elteq!$F$5)","v":17.512231905994774}]
["ANAMET-M",2655210,"MSV PG 21 B-23","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,26.430928261302459,{"$f":"F2551*(1-Elteq!$F$5)","v":26.430928261302459}]
["ANAMET-M",2655290,"MSV PG 29 B-29","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,29.450278589922249,{"$f":"F2552*(1-Elteq!$F$5)","v":29.450278589922249}]
["ANAMET-M",2655360,"MSV PG 36 B-36","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,51.180310647281289,{"$f":"F2553*(1-Elteq!$F$5)","v":51.180310647281289}]
["ANAMET-M",2655480,"MSV PG 48 B-48","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",1,70.104669476199774,{"$f":"F2554*(1-Elteq!$F$5)","v":70.104669476199774}]
["ANAMET-M",2657090,"MSV 90 PG 9 B-10","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,16.824749061939809,{"$f":"F2555*(1-Elteq!$F$5)","v":16.824749061939809}]
["ANAMET-M",2657110,"MSV 90 PG 11 B-12","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,16.824749061939809,{"$f":"F2556*(1-Elteq!$F$5)","v":16.824749061939809}]
["ANAMET-M",2657130,"MSV 90 PG 13 B-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,18.524875554670338,{"$f":"F2557*(1-Elteq!$F$5)","v":18.524875554670338}]
["ANAMET-M",2657160,"MSV 90 PG 16 B-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,19.723325377414806,{"$f":"F2558*(1-Elteq!$F$5)","v":19.723325377414806}]
["ANAMET-M",2657210,"MSV 90 PG 21 B-23","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,26.728218139812714,{"$f":"F2559*(1-Elteq!$F$5)","v":26.728218139812714}]
["ANAMET-M",2657290,"MSV 90 PG 29 B-29","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,30.044858346942764,{"$f":"F2560*(1-Elteq!$F$5)","v":30.044858346942764}]
["ANAMET-M",2657360,"MSV 90 PG 36 B-36","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,56.605850930093453,{"$f":"F2561*(1-Elteq!$F$5)","v":56.605850930093453}]
["ANAMET-M",2657480,"MSV 90 PG 48 B-48","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",1,86.241935694084617,{"$f":"F2562*(1-Elteq!$F$5)","v":86.241935694084617}]
["ANAMET-M",2672070,"CH NW 7,5 G","Fittings for Anaquick conduit, Conduit holder",1,1.1334176618203515,{"$f":"F2563*(1-Elteq!$F$5)","v":1.1334176618203515}]
["ANAMET-M",2672100,"CH NW 10 G","Fittings for Anaquick conduit, Conduit holder",1,1.1891595140410245,{"$f":"F2564*(1-Elteq!$F$5)","v":1.1891595140410245}]
["ANAMET-M",2672120,"CH NW 12 G","Fittings for Anaquick conduit, Conduit holder",1,1.3563850707030436,{"$f":"F2565*(1-Elteq!$F$5)","v":1.3563850707030436}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},2672170,"CH NW 17 G","Fittings for Anaquick conduit, Conduit holder",1,1.421417231627162,{"$f":"F2566*(1-Elteq!$F$5)","v":1.421417231627162}]
["ANAMET-M",2672230,"CH NW 23 G","Fittings for Anaquick conduit, Conduit holder",1,2.1925128540131387,{"$f":"F2567*(1-Elteq!$F$5)","v":2.1925128540131387}]
["ANAMET-M",2672290,"CH NW 29 G","Fittings for Anaquick conduit, Conduit holder",1,2.5362542760406228,{"$f":"F2568*(1-Elteq!$F$5)","v":2.5362542760406228}]
["ANAMET-M",2672360,"CH NW 37 G","Fittings for Anaquick conduit, Conduit holder",1,3.5488979247161825,{"$f":"F2569*(1-Elteq!$F$5)","v":3.5488979247161825}]
["ANAMET-M",2672480,"CH NW 50 G","Fittings for Anaquick conduit, Conduit holder",1,4.3199935471021602,{"$f":"F2570*(1-Elteq!$F$5)","v":4.3199935471021602}]
["ANAMET-M",2673070,"CH NW 7,5 B","Fittings for Anaquick conduit, Conduit holder",1,1.1334176618203515,{"$f":"F2571*(1-Elteq!$F$5)","v":1.1334176618203515}]
["ANAMET-M",2673100,"CH NW 10 B","Fittings for Anaquick conduit, Conduit holder",1,1.1891595140410245,{"$f":"F2572*(1-Elteq!$F$5)","v":1.1891595140410245}]
["ANAMET-M",2673120,"CH NW 12 B","Fittings for Anaquick conduit, Conduit holder",1,1.3563850707030436,{"$f":"F2573*(1-Elteq!$F$5)","v":1.3563850707030436}]
["ANAMET-M",2673170,"CH NW 17 B","Fittings for Anaquick conduit, Conduit holder",1,1.421417231627162,{"$f":"F2574*(1-Elteq!$F$5)","v":1.421417231627162}]
["ANAMET-M",2673230,"CH NW 23 B","Fittings for Anaquick conduit, Conduit holder",1,2.1925128540131387,{"$f":"F2575*(1-Elteq!$F$5)","v":2.1925128540131387}]
["ANAMET-M",2673290,"CH NW 29 B","Fittings for Anaquick conduit, Conduit holder",1,2.5362542760406228,{"$f":"F2576*(1-Elteq!$F$5)","v":2.5362542760406228}]
["ANAMET-M",2673360,"CH NW 37 B","Fittings for Anaquick conduit, Conduit holder",1,3.5488979247161825,{"$f":"F2577*(1-Elteq!$F$5)","v":3.5488979247161825}]
["ANAMET-M",2673480,"CH NW 50 B","Fittings for Anaquick conduit, Conduit holder",1,4.3199935471021602,{"$f":"F2578*(1-Elteq!$F$5)","v":4.3199935471021602}]
["ANAMET-M",2674070,"CC NW 7,5 G","Fittings for Anaquick conduit, Conduit holder cover",1,0.70606346146185839,{"$f":"F2579*(1-Elteq!$F$5)","v":0.70606346146185839}]
["ANAMET-M",2674100,"CC NW 10 G","Fittings for Anaquick conduit, Conduit holder cover",1,0.70606346146185839,{"$f":"F2580*(1-Elteq!$F$5)","v":0.70606346146185839}]
["ANAMET-M",2674120,"CC NW 12 G","Fittings for Anaquick conduit, Conduit holder cover",1,0.8268374746066498,{"$f":"F2581*(1-Elteq!$F$5)","v":0.8268374746066498}]
["ANAMET-M",2674170,"CC NW 17 G","Fittings for Anaquick conduit, Conduit holder cover",1,0.8268374746066498,{"$f":"F2582*(1-Elteq!$F$5)","v":0.8268374746066498}]
["ANAMET-M",2674230,"CC NW 23 G","Fittings for Anaquick conduit, Conduit holder cover",1,1.0126436486755599,{"$f":"F2583*(1-Elteq!$F$5)","v":1.0126436486755599}]
["ANAMET-M",2674290,"CC NW 29 G","Fittings for Anaquick conduit, Conduit holder cover",1,1.0126436486755599,{"$f":"F2584*(1-Elteq!$F$5)","v":1.0126436486755599}]
["ANAMET-M",2674360,"CC NW 37 G","Fittings for Anaquick conduit, Conduit holder cover",1,1.1334176618203515,{"$f":"F2585*(1-Elteq!$F$5)","v":1.1334176618203515}]
["ANAMET-M",2674480,"CC NW 50 G","Fittings for Anaquick conduit, Conduit holder cover",1,1.1334176618203515,{"$f":"F2586*(1-Elteq!$F$5)","v":1.1334176618203515}]
["ANAMET-M",2675000,"CH CON - G","Fittings for Anaquick conduit, Conduit holder cover",1,0.24154802628958311,{"$f":"F2587*(1-Elteq!$F$5)","v":0.24154802628958311}]
["ANAMET-M",2675010,"CH CON - B","Fittings for Anaquick conduit, Conduit holder cover",1,0.24154802628958311,{"$f":"F2588*(1-Elteq!$F$5)","v":0.24154802628958311}]
["ANAMET-M",2675070,"CC NW 7,5 B","Fittings for Anaquick conduit, Conduit holder cover",1,0.70606346146185839,{"$f":"F2589*(1-Elteq!$F$5)","v":0.70606346146185839}]
["ANAMET-M",2675100,"CC NW 10 B","Fittings for Anaquick conduit, Conduit holder cover",1,0.70606346146185839,{"$f":"F2590*(1-Elteq!$F$5)","v":0.70606346146185839}]
["ANAMET-M",2675120,"CC NW 12 B","Fittings for Anaquick conduit, Conduit holder cover",1,0.8268374746066498,{"$f":"F2591*(1-Elteq!$F$5)","v":0.8268374746066498}]
["ANAMET-M",2675170,"CC NW 17 B","Fittings for Anaquick conduit, Conduit holder cover",1,0.8268374746066498,{"$f":"F2592*(1-Elteq!$F$5)","v":0.8268374746066498}]
["ANAMET-M",2675230,"CC NW 23 B","Fittings for Anaquick conduit, Conduit holder cover",1,1.0126436486755599,{"$f":"F2593*(1-Elteq!$F$5)","v":1.0126436486755599}]
["ANAMET-M",2675290,"CC NW 29 B","Fittings for Anaquick conduit, Conduit holder cover",1,1.0126436486755599,{"$f":"F2594*(1-Elteq!$F$5)","v":1.0126436486755599}]
["ANAMET-M",2675360,"CC NW 37 B","Fittings for Anaquick conduit, Conduit holder cover",1,1.1334176618203515,{"$f":"F2595*(1-Elteq!$F$5)","v":1.1334176618203515}]
["ANAMET-M",2675480,"CC NW 50 B","Fittings for Anaquick conduit, Conduit holder cover",1,1.1334176618203515,{"$f":"F2596*(1-Elteq!$F$5)","v":1.1334176618203515}]
["ANAMET-M",2676100,"CLIP NW 10 B","Fittings for Anaquick conduit, Conduit clip",1,6.4660548575980705,{"$f":"F2597*(1-Elteq!$F$5)","v":6.4660548575980705}]
["ANAMET-M",2676130,"CLIP NW 13 B","Fittings for Anaquick conduit, Conduit clip",1,6.6146997968531984,{"$f":"F2598*(1-Elteq!$F$5)","v":6.6146997968531984}]
["ANAMET-M",2676170,"CLIP NW 17 B","Fittings for Anaquick conduit, Conduit clip",1,6.939860601473792,{"$f":"F2599*(1-Elteq!$F$5)","v":6.939860601473792}]
["ANAMET-M",2676220,"CLIP NW 22 B","Fittings for Anaquick conduit, Conduit clip",1,7.097795849432365,{"$f":"F2600*(1-Elteq!$F$5)","v":7.097795849432365}]
["ANAMET-M",2677100,"NW 10","Fittings for Anaquick conduit, Conduit reducer",1,0.27870926110336514,{"$f":"F2601*(1-Elteq!$F$5)","v":0.27870926110336514}]
["ANAMET-M",2677110,"NW 10","Fittings for Anaquick conduit, Conduit reducer",1,0.28799956980681063,{"$f":"F2602*(1-Elteq!$F$5)","v":0.28799956980681063}]
["ANAMET-M",2677130,"NW 13","Fittings for Anaquick conduit, Conduit reducer",1,0.28799956980681063,{"$f":"F2603*(1-Elteq!$F$5)","v":0.28799956980681063}]
["ANAMET-M",2677140,"NW 13","Fittings for Anaquick conduit, Conduit reducer",1,0.29728987851025612,{"$f":"F2604*(1-Elteq!$F$5)","v":0.29728987851025612}]
["ANAMET-M",2677170,"NW 17","Fittings for Anaquick conduit, Conduit reducer",1,0.38090265684126562,{"$f":"F2605*(1-Elteq!$F$5)","v":0.38090265684126562}]
["ANAMET-M",2678170,"NW 17","Fittings for Anaquick conduit, Conduit reducer",1,0.23225771758613761,{"$f":"F2606*(1-Elteq!$F$5)","v":0.23225771758613761}]
["ANAMET-M",2678200,"NW 22","Fittings for Anaquick conduit, Conduit reducer",1,0.26941895239991959,{"$f":"F2607*(1-Elteq!$F$5)","v":0.26941895239991959}]
["ANAMET-M",2678210,"NW 22","Fittings for Anaquick conduit, Conduit reducer",1,0.39948327424815672,{"$f":"F2608*(1-Elteq!$F$5)","v":0.39948327424815672}]
["ANAMET-M",2678220,"NW 22","Fittings for Anaquick conduit, Conduit reducer",1,0.90115994423421386,{"$f":"F2609*(1-Elteq!$F$5)","v":0.90115994423421386}]
["ANAMET-M",7977010,"T 7-7-7","Fittings for Anaquick conduit, T-joint splitable, IP 40",1,0.53883790479983917,{"$f":"F2610*(1-Elteq!$F$5)","v":0.53883790479983917}]
["ANAMET-M",7977020,"T 10-7-7","Fittings for Anaquick conduit, T-joint splitable, IP 40",1,0.99406303126866913,{"$f":"F2611*(1-Elteq!$F$5)","v":0.99406303126866913}]
["ANAMET-M",7977030,"T 10-10-7","Fittings for Anaquick conduit, T-joint splitable, IP 40",1,0.48309605257916621,{"$f":"F2612*(1-Elteq!$F$5)","v":0.48309605257916621}]
["ANAMET-M",7977040,"T 10-10-10","Fittings for Anaquick conduit, T-joint splitable, IP 40",1,0.48309605257916621,{"$f":"F2613*(1-Elteq!$F$5)","v":0.48309605257916621}]
["ANAMET-M",7977050,"T 12-12-7","Fittings for Anaquick conduit, T-joint splitable, IP 40",1,0.5202572873929483,{"$f":"F2614*(1-Elteq!$F$5)","v":0.5202572873929483}]
["ANAMET-M",7977060,"T 12-10-10","Fittings for Anaquick conduit, T-joint splitable, IP 40",1,0.78038593108942222,{"$f":"F2615*(1-Elteq!$F$5)","v":0.78038593108942222}]
["ANAMET-M",7977070,"T 17-10-17","Fittings for Anaquick conduit, T-joint splitable, IP 40",1,0.60387006572395774,{"$f":"F2616*(1-Elteq!$F$5)","v":0.60387006572395774}]
["ANAMET-M",7977080,"T 17-12-12","Fittings for Anaquick conduit, T-joint splitable, IP 40",1,0.62245068313084884,{"$f":"F2617*(1-Elteq!$F$5)","v":0.62245068313084884}]
["ANAMET-M",7977090,"T 17-12-17","Fittings for Anaquick conduit, T-joint splitable, IP 40",1,0.6781925353515218,{"$f":"F2618*(1-Elteq!$F$5)","v":0.6781925353515218}]
["ANAMET-M",7977100,"T 17-23-17","Fittings for Anaquick conduit, T-joint splitable, IP 40",1,0.8268374746066498,{"$f":"F2619*(1-Elteq!$F$5)","v":0.8268374746066498}]
["ANAMET-M",7977110,"T 23-10-23","Fittings for Anaquick conduit, T-joint splitable, IP 40",1,2.0438679147580112,{"$f":"F2620*(1-Elteq!$F$5)","v":2.0438679147580112}]
["ANAMET-M",7977120,"T 23-12-23","Fittings for Anaquick conduit, T-joint splitable, IP 40",1,1.0126436486755599,{"$f":"F2621*(1-Elteq!$F$5)","v":1.0126436486755599}]
["ANAMET-M",7977130,"T 23-17-12","Fittings for Anaquick conduit, T-joint splitable, IP 40",1,0.85470840071698639,{"$f":"F2622*(1-Elteq!$F$5)","v":0.85470840071698639}]
["ANAMET-M",7977140,"T 23-23-10","Fittings for Anaquick conduit, T-joint splitable, IP 40",1,0.98477272256522352,{"$f":"F2623*(1-Elteq!$F$5)","v":0.98477272256522352}]
["ANAMET-M",7977150,"T 23-23-23","Fittings for Anaquick conduit, T-joint splitable, IP 40",1,1.6536749492132996,{"$f":"F2624*(1-Elteq!$F$5)","v":1.6536749492132996}]
["ANAMET-M",7978010,"Y 12-10-10","Fittings for Anaquick conduit, Y-joint splitable, IP 40",1,1.1055467357100148,{"$f":"F2625*(1-Elteq!$F$5)","v":1.1055467357100148}]
["ANAMET-M",7978020,"Y 12-10-12","Fittings for Anaquick conduit, Y-joint splitable, IP 40",1,1.1055467357100148,{"$f":"F2626*(1-Elteq!$F$5)","v":1.1055467357100148}]
["ANAMET-M",7978030,"Y 12-12-12","Fittings for Anaquick conduit, Y-joint splitable, IP 40",1,1.1055467357100148,{"$f":"F2627*(1-Elteq!$F$5)","v":1.1055467357100148}]
["ANAMET-M",7978040,"Y 17-10-10","Fittings for Anaquick conduit, Y-joint splitable, IP 40",1,0.81754716590320442,{"$f":"F2628*(1-Elteq!$F$5)","v":0.81754716590320442}]
["ANAMET-M",7978050,"Y 17-10-17","Fittings for Anaquick conduit, Y-joint splitable, IP 40",1,0.93832117904799595,{"$f":"F2629*(1-Elteq!$F$5)","v":0.93832117904799595}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},7978060,"Y 17-12-10","Fittings for Anaquick conduit, Y-joint splitable, IP 40",1,1.2263207488548067,{"$f":"F2630*(1-Elteq!$F$5)","v":1.2263207488548067}]
["ANAMET-M",7978070,"Y 17-12-12","Fittings for Anaquick conduit, Y-joint splitable, IP 40",1,0.83612778331009541,{"$f":"F2631*(1-Elteq!$F$5)","v":0.83612778331009541}]
["ANAMET-M",7978080,"Y 17-17-10","Fittings for Anaquick conduit, Y-joint splitable, IP 40",1,1.2263207488548067,{"$f":"F2632*(1-Elteq!$F$5)","v":1.2263207488548067}]
["ANAMET-M",7978090,"Y 23-10-23","Fittings for Anaquick conduit, Y-joint splitable, IP 40",1,1.3285141445927069,{"$f":"F2633*(1-Elteq!$F$5)","v":1.3285141445927069}]
["ANAMET-M",7978100,"Y 23-12-23","Fittings for Anaquick conduit, Y-joint splitable, IP 40",1,1.2820626010754794,{"$f":"F2634*(1-Elteq!$F$5)","v":1.2820626010754794}]
["ANAMET-M",7978110,"Y 23-23-23","Fittings for Anaquick conduit, Y-joint splitable, IP 40",1,1.4028366142202711,{"$f":"F2635*(1-Elteq!$F$5)","v":1.4028366142202711}]
["ANAMET-M",7998010,"T 10-10-10","Fittings for Anaquick conduit, T-joint conduit",1,0.8268374746066498,{"$f":"F2636*(1-Elteq!$F$5)","v":0.8268374746066498}]
["ANAMET-M",7998020,"T 17-17-10","Fittings for Anaquick conduit, T-joint conduit",1,0.56670883091017576,{"$f":"F2637*(1-Elteq!$F$5)","v":0.56670883091017576}]
["ANAMET-M",7998030,"T 17-17-17","Fittings for Anaquick conduit, T-joint conduit",1,1.1055467357100148,{"$f":"F2638*(1-Elteq!$F$5)","v":1.1055467357100148}]
["ANAMET-M",7998040,"T 23-23-10","Fittings for Anaquick conduit, T-joint conduit",1,1.7372877275443095,{"$f":"F2639*(1-Elteq!$F$5)","v":1.7372877275443095}]
["ANAMET-M",7998050,"T 23-23-17","Fittings for Anaquick conduit, T-joint conduit",1,2.2482547062338121,{"$f":"F2640*(1-Elteq!$F$5)","v":2.2482547062338121}]
["ANAMET-M",7998060,"T 23-23-23","Fittings for Anaquick conduit, T-joint conduit",1,1.7372877275443095,{"$f":"F2641*(1-Elteq!$F$5)","v":1.7372877275443095}]
["ANAMET-M",7998070,"T 10-17-23","Fittings for Anaquick conduit, T-joint conduit",1,1.5421912447719537,{"$f":"F2642*(1-Elteq!$F$5)","v":1.5421912447719537}]
["ANAMET-M",2699070,"CN 7 G","Fittings for Anaquick conduit, Locknut, polyamide",1,0.16722555666201905,{"$f":"F2643*(1-Elteq!$F$5)","v":0.16722555666201905}]
["ANAMET-M",2699073,"CN 7 B","Fittings for Anaquick conduit, Locknut, polyamide",1,0.16722555666201905,{"$f":"F2644*(1-Elteq!$F$5)","v":0.16722555666201905}]
["ANAMET-M",2699090,"CN 9 G","Fittings for Anaquick conduit, Locknut, polyamide",1,0.16722555666201905,{"$f":"F2645*(1-Elteq!$F$5)","v":0.16722555666201905}]
["ANAMET-M",2699093,"CN 9 B","Fittings for Anaquick conduit, Locknut, polyamide",1,0.16722555666201905,{"$f":"F2646*(1-Elteq!$F$5)","v":0.16722555666201905}]
["ANAMET-M",2699110,"CN 11 G","Fittings for Anaquick conduit, Locknut, polyamide",1,0.16722555666201905,{"$f":"F2647*(1-Elteq!$F$5)","v":0.16722555666201905}]
["ANAMET-M",2699113,"CN 11 B","Fittings for Anaquick conduit, Locknut, polyamide",1,0.16722555666201905,{"$f":"F2648*(1-Elteq!$F$5)","v":0.16722555666201905}]
["ANAMET-M",2699130,"CN 13 G","Fittings for Anaquick conduit, Locknut, polyamide",1,0.22296740888269209,{"$f":"F2649*(1-Elteq!$F$5)","v":0.22296740888269209}]
["ANAMET-M",2699133,"CN 13 B","Fittings for Anaquick conduit, Locknut, polyamide",1,0.22296740888269209,{"$f":"F2650*(1-Elteq!$F$5)","v":0.22296740888269209}]
["ANAMET-M",2699160,"CN 16 G","Fittings for Anaquick conduit, Locknut, polyamide",1,0.22296740888269209,{"$f":"F2651*(1-Elteq!$F$5)","v":0.22296740888269209}]
["ANAMET-M",2699163,"CN 16 B","Fittings for Anaquick conduit, Locknut, polyamide",1,0.22296740888269209,{"$f":"F2652*(1-Elteq!$F$5)","v":0.22296740888269209}]
["ANAMET-M",2699210,"CN 21 G","Fittings for Anaquick conduit, Locknut, polyamide",1,0.39948327424815672,{"$f":"F2653*(1-Elteq!$F$5)","v":0.39948327424815672}]
["ANAMET-M",2699213,"CN 21 B","Fittings for Anaquick conduit, Locknut, polyamide",1,0.39948327424815672,{"$f":"F2654*(1-Elteq!$F$5)","v":0.39948327424815672}]
["ANAMET-M",2699290,"CN 29 G","Fittings for Anaquick conduit, Locknut, polyamide",1,0.70606346146185839,{"$f":"F2655*(1-Elteq!$F$5)","v":0.70606346146185839}]
["ANAMET-M",2699293,"CN 29 B","Fittings for Anaquick conduit, Locknut, polyamide",1,0.70606346146185839,{"$f":"F2656*(1-Elteq!$F$5)","v":0.70606346146185839}]
["ANAMET-M",2699360,"CN 36 G","Fittings for Anaquick conduit, Locknut, polyamide",1,1.5050300099581719,{"$f":"F2657*(1-Elteq!$F$5)","v":1.5050300099581719}]
["ANAMET-M",2699363,"CN 36 B","Fittings for Anaquick conduit, Locknut, polyamide",1,1.5050300099581719,{"$f":"F2658*(1-Elteq!$F$5)","v":1.5050300099581719}]
["ANAMET-M",2699480,"CN 48 G","Fittings for Anaquick conduit, Locknut, polyamide",1,2.2575450149372576,{"$f":"F2659*(1-Elteq!$F$5)","v":2.2575450149372576}]
["ANAMET-M",2699483,"CN 48 B","Fittings for Anaquick conduit, Locknut, polyamide",1,2.2575450149372576,{"$f":"F2660*(1-Elteq!$F$5)","v":2.2575450149372576}]
["ANAMET-M",7983120,"CN M 12 G","Fittings for Anaquick conduit, Locknut, polyamide",1,0.16722555666201905,{"$f":"F2661*(1-Elteq!$F$5)","v":0.16722555666201905}]
["ANAMET-M",7983123,"CN M 12 B","Fittings for Anaquick conduit, Locknut, polyamide",1,0.16722555666201905,{"$f":"F2662*(1-Elteq!$F$5)","v":0.16722555666201905}]
["ANAMET-M",7983160,"CN M 16 G","Fittings for Anaquick conduit, Locknut, polyamide",1,0.22296740888269209,{"$f":"F2663*(1-Elteq!$F$5)","v":0.22296740888269209}]
["ANAMET-M",7983163,"CN M 16 B","Fittings for Anaquick conduit, Locknut, polyamide",1,0.22296740888269209,{"$f":"F2664*(1-Elteq!$F$5)","v":0.22296740888269209}]
["ANAMET-M",7983200,"CN M 20 G","Fittings for Anaquick conduit, Locknut, polyamide",1,0.22296740888269209,{"$f":"F2665*(1-Elteq!$F$5)","v":0.22296740888269209}]
["ANAMET-M",7983203,"CN M 20 B","Fittings for Anaquick conduit, Locknut, polyamide",1,0.22296740888269209,{"$f":"F2666*(1-Elteq!$F$5)","v":0.22296740888269209}]
["ANAMET-M",7983250,"CN M 25 G","Fittings for Anaquick conduit, Locknut, polyamide",1,0.30658018721370167,{"$f":"F2667*(1-Elteq!$F$5)","v":0.30658018721370167}]
["ANAMET-M",7983253,"CN M 25 B","Fittings for Anaquick conduit, Locknut, polyamide",1,0.30658018721370167,{"$f":"F2668*(1-Elteq!$F$5)","v":0.30658018721370167}]
["ANAMET-M",7983320,"CN M 32 G","Fittings for Anaquick conduit, Locknut, polyamide",1,0.59457975702051225,{"$f":"F2669*(1-Elteq!$F$5)","v":0.59457975702051225}]
["ANAMET-M",7983323,"CN M 32 B","Fittings for Anaquick conduit, Locknut, polyamide",1,0.59457975702051225,{"$f":"F2670*(1-Elteq!$F$5)","v":0.59457975702051225}]
["ANAMET-M",7983400,"CN M 40 G","Fittings for Anaquick conduit, Locknut, polyamide",1,0.96619210515833243,{"$f":"F2671*(1-Elteq!$F$5)","v":0.96619210515833243}]
["ANAMET-M",7983403,"CN M 40 B","Fittings for Anaquick conduit, Locknut, polyamide",1,0.96619210515833243,{"$f":"F2672*(1-Elteq!$F$5)","v":0.96619210515833243}]
["ANAMET-M",7983500,"CN M 50 G","Fittings for Anaquick conduit, Locknut, polyamide",1,1.5979330969926269,{"$f":"F2673*(1-Elteq!$F$5)","v":1.5979330969926269}]
["ANAMET-M",7983503,"CN M 50 B","Fittings for Anaquick conduit, Locknut, polyamide",1,1.5979330969926269,{"$f":"F2674*(1-Elteq!$F$5)","v":1.5979330969926269}]
["ANAMET-M",7983630,"CN M 63 G","Fittings for Anaquick conduit, Locknut, polyamide",1,2.39689964548894,{"$f":"F2675*(1-Elteq!$F$5)","v":2.39689964548894}]
["ANAMET-M",7983633,"CN M 63 B","Fittings for Anaquick conduit, Locknut, polyamide",1,2.39689964548894,{"$f":"F2676*(1-Elteq!$F$5)","v":2.39689964548894}]
["ANAMET-M",2661090,"PG 9","Fittings for Anaquick conduit, Reducer Pg/PG polyamide",1,1.0869661183031241,{"$f":"F2677*(1-Elteq!$F$5)","v":1.0869661183031241}]
["ANAMET-M",2661110,"PG 11","Fittings for Anaquick conduit, Reducer Pg/PG polyamide",1,1.0312242660824511,{"$f":"F2678*(1-Elteq!$F$5)","v":1.0312242660824511}]
["ANAMET-M",2661150,"PG16","Fittings for Anaquick conduit, Reducer Pg/PG polyamide",1,1.3285141445927069,{"$f":"F2679*(1-Elteq!$F$5)","v":1.3285141445927069}]
["ANAMET-M",2661160,"PG 16","Fittings for Anaquick conduit, Reducer Pg/PG polyamide",1,1.2263207488548067,{"$f":"F2680*(1-Elteq!$F$5)","v":1.2263207488548067}]
["ANAMET-M",2661210,"PG 21","Fittings for Anaquick conduit, Reducer Pg/PG polyamide",1,1.8209005058753187,{"$f":"F2681*(1-Elteq!$F$5)","v":1.8209005058753187}]
["ANAMET-M",2661290,"PG 29","Fittings for Anaquick conduit, Reducer Pg/PG polyamide",1,3.7254137900816469,{"$f":"F2682*(1-Elteq!$F$5)","v":3.7254137900816469}]
["ANAMET-M",2661360,"PG 36","Fittings for Anaquick conduit, Reducer Pg/PG polyamide",1,4.1341873730332495,{"$f":"F2683*(1-Elteq!$F$5)","v":4.1341873730332495}]
["ANAMET-M",2661420,"PG 42","Fittings for Anaquick conduit, Reducer Pg/PG polyamide",1,9.2531474686317221,{"$f":"F2684*(1-Elteq!$F$5)","v":9.2531474686317221}]
["ANAMET-M",2661480,"PG 48","Fittings for Anaquick conduit, Reducer Pg/PG polyamide",1,11.5757246444931,{"$f":"F2685*(1-Elteq!$F$5)","v":11.5757246444931}]
["ANAMET-M",2662070,"PG 7","Fittings for Anaquick conduit, Enlarger Pg/PG polyamide",1,0.81754716590320442,{"$f":"F2686*(1-Elteq!$F$5)","v":0.81754716590320442}]
["ANAMET-M",2662090,"PG 9","Fittings for Anaquick conduit, Enlarger Pg/PG polyamide",1,0.93832117904799595,{"$f":"F2687*(1-Elteq!$F$5)","v":0.93832117904799595}]
["ANAMET-M",2662110,"PG 11","Fittings for Anaquick conduit, Enlarger Pg/PG polyamide",1,1.1148370444134605,{"$f":"F2688*(1-Elteq!$F$5)","v":1.1148370444134605}]
["ANAMET-M",2662160,"PG 16","Fittings for Anaquick conduit, Enlarger Pg/PG polyamide",1,1.8209005058753187,{"$f":"F2689*(1-Elteq!$F$5)","v":1.8209005058753187}]
["ANAMET-M",2662210,"PG 21","Fittings for Anaquick conduit, Enlarger Pg/PG polyamide",1,3.7439944074885387,{"$f":"F2690*(1-Elteq!$F$5)","v":3.7439944074885387}]
["ANAMET-M",2662290,"PG29","Fittings for Anaquick conduit, Enlarger Pg/PG polyamide",1,6.5961191794463083,{"$f":"F2691*(1-Elteq!$F$5)","v":6.5961191794463083}]
["ANAMET-M",2662360,"PG 36","Fittings for Anaquick conduit, Enlarger Pg/PG polyamide",1,9.7269532125074427,{"$f":"F2692*(1-Elteq!$F$5)","v":9.7269532125074427}]
["ANAMET-M",2662420,"PG 42","Fittings for Anaquick conduit, Enlarger Pg/PG polyamide",1,12.718432615016894,{"$f":"F2693*(1-Elteq!$F$5)","v":12.718432615016894}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},2664160,"M16","Fittings for Anaquick conduit, Reducer ISO/ISO polyamide",1,0.68748284405496729,{"$f":"F2694*(1-Elteq!$F$5)","v":0.68748284405496729}]
["ANAMET-M",2664200,"M20","Fittings for Anaquick conduit, Reducer ISO/ISO polyamide",1,0.73393438757219487,{"$f":"F2695*(1-Elteq!$F$5)","v":0.73393438757219487}]
["ANAMET-M",2664250,"M25","Fittings for Anaquick conduit, Reducer ISO/ISO polyamide",1,0.8268374746066498,{"$f":"F2696*(1-Elteq!$F$5)","v":0.8268374746066498}]
["ANAMET-M",2664320,"M32","Fittings for Anaquick conduit, Reducer ISO/ISO polyamide",1,1.0312242660824511,{"$f":"F2697*(1-Elteq!$F$5)","v":1.0312242660824511}]
["ANAMET-M",2664400,"M40","Fittings for Anaquick conduit, Reducer ISO/ISO polyamide",1,1.6258040231029631,{"$f":"F2698*(1-Elteq!$F$5)","v":1.6258040231029631}]
["ANAMET-M",2664500,"M50","Fittings for Anaquick conduit, Reducer ISO/ISO polyamide",1,3.4467045289782821,{"$f":"F2699*(1-Elteq!$F$5)","v":3.4467045289782821}]
["ANAMET-M",2664630,"M63","Fittings for Anaquick conduit, Reducer ISO/ISO polyamide",1,4.1992195339573675,{"$f":"F2700*(1-Elteq!$F$5)","v":4.1992195339573675}]
["ANAMET-M",2665120,"M12","Fittings for Anaquick conduit, Enlarger ISO/ISO polyamide",1,0.74322469627564036,{"$f":"F2701*(1-Elteq!$F$5)","v":0.74322469627564036}]
["ANAMET-M",2665160,"M16","Fittings for Anaquick conduit, Enlarger ISO/ISO polyamide",1,0.91045025293765935,{"$f":"F2702*(1-Elteq!$F$5)","v":0.91045025293765935}]
["ANAMET-M",2665200,"M20","Fittings for Anaquick conduit, Enlarger ISO/ISO polyamide",1,0.93832117904799595,{"$f":"F2703*(1-Elteq!$F$5)","v":0.93832117904799595}]
["ANAMET-M",2665250,"M25","Fittings for Anaquick conduit, Enlarger ISO/ISO polyamide",1,1.0405145747858966,{"$f":"F2704*(1-Elteq!$F$5)","v":1.0405145747858966}]
["ANAMET-M",2665320,"M32","Fittings for Anaquick conduit, Enlarger ISO/ISO polyamide",1,1.5329009360685082,{"$f":"F2705*(1-Elteq!$F$5)","v":1.5329009360685082}]
["ANAMET-M",2665400,"M40","Fittings for Anaquick conduit, Enlarger ISO/ISO polyamide",1,3.0193503286197889,{"$f":"F2706*(1-Elteq!$F$5)","v":3.0193503286197889}]
["ANAMET-M",2665500,"M50","Fittings for Anaquick conduit, Enlarger ISO/ISO polyamide",1,4.1806389165504774,{"$f":"F2707*(1-Elteq!$F$5)","v":4.1806389165504774}]
["ANAMET-M",2666120,"M12","Fittings for Anaquick conduit, Blindplug ISO polyamide",1,0.3344511133240381,{"$f":"F2708*(1-Elteq!$F$5)","v":0.3344511133240381}]
["ANAMET-M",2666160,"M16","Fittings for Anaquick conduit, Blindplug ISO polyamide",1,0.38090265684126562,{"$f":"F2709*(1-Elteq!$F$5)","v":0.38090265684126562}]
["ANAMET-M",2666200,"M20","Fittings for Anaquick conduit, Blindplug ISO polyamide",1,0.44593481776538418,{"$f":"F2710*(1-Elteq!$F$5)","v":0.44593481776538418}]
["ANAMET-M",2666250,"M25","Fittings for Anaquick conduit, Blindplug ISO polyamide",1,0.56670883091017576,{"$f":"F2711*(1-Elteq!$F$5)","v":0.56670883091017576}]
["ANAMET-M",2666320,"M32","Fittings for Anaquick conduit, Blindplug ISO polyamide",1,1.0405145747858966,{"$f":"F2712*(1-Elteq!$F$5)","v":1.0405145747858966}]
["ANAMET-M",2666400,"M40","Fittings for Anaquick conduit, Blindplug ISO polyamide",1,1.3099335271858161,{"$f":"F2713*(1-Elteq!$F$5)","v":1.3099335271858161}]
["ANAMET-M",2666500,"M50","Fittings for Anaquick conduit, Blindplug ISO polyamide",1,2.2761256323441486,{"$f":"F2714*(1-Elteq!$F$5)","v":2.2761256323441486}]
["ANAMET-M",2666630,"M63","Fittings for Anaquick conduit, Blindplug ISO polyamide",1,3.3352208245369357,{"$f":"F2715*(1-Elteq!$F$5)","v":3.3352208245369357}]
["ANAMET-M",2667070,"PG 7","Fittings for Anaquick conduit, Blindplug PG polyamide",1,0.88257932682732287,{"$f":"F2716*(1-Elteq!$F$5)","v":0.88257932682732287}]
["ANAMET-M",2667090,"PG 9","Fittings for Anaquick conduit, Blindplug PG polyamide",1,0.88257932682732287,{"$f":"F2717*(1-Elteq!$F$5)","v":0.88257932682732287}]
["ANAMET-M",2667110,"PG 11","Fittings for Anaquick conduit, Blindplug PG polyamide",1,0.96619210515833243,{"$f":"F2718*(1-Elteq!$F$5)","v":0.96619210515833243}]
["ANAMET-M",2667130,"PG13,5","Fittings for Anaquick conduit, Blindplug PG polyamide",1,1.0219339573790056,{"$f":"F2719*(1-Elteq!$F$5)","v":1.0219339573790056}]
["ANAMET-M",2667160,"PG 16","Fittings for Anaquick conduit, Blindplug PG polyamide",1,1.1427079705237968,{"$f":"F2720*(1-Elteq!$F$5)","v":1.1427079705237968}]
["ANAMET-M",2667210,"PG 21","Fittings for Anaquick conduit, Blindplug PG polyamide",1,1.5514815534753992,{"$f":"F2721*(1-Elteq!$F$5)","v":1.5514815534753992}]
["ANAMET-M",2667290,"PG29","Fittings for Anaquick conduit, Blindplug PG polyamide",1,2.8614150806612151,{"$f":"F2722*(1-Elteq!$F$5)","v":2.8614150806612151}]
["ANAMET-M",2667360,"PG 36","Fittings for Anaquick conduit, Blindplug PG polyamide",1,6.2152165226050426,{"$f":"F2723*(1-Elteq!$F$5)","v":6.2152165226050426}]
["ANAMET-M",2667480,"PG 48","Fittings for Anaquick conduit, Blindplug PG polyamide",1,8.4356003027285169,{"$f":"F2724*(1-Elteq!$F$5)","v":8.4356003027285169}]
["ANAMET-M",2690703,"70 mm","Fittings for gigant conduit, Straight fixed with flange, IP 54",1,24.953769177454625,{"$f":"F2725*(1-Elteq!$F$5)","v":24.953769177454625}]
["ANAMET-M",2690993,"95 mm","Fittings for gigant conduit, Straight fixed with flange, IP 54",1,30.518664090818483,{"$f":"F2726*(1-Elteq!$F$5)","v":30.518664090818483}]
["ANAMET-M",2691703,"70 mm","Fittings for gigant conduit, Straight fixed with flange, IP 54",1,24.953769177454625,{"$f":"F2727*(1-Elteq!$F$5)","v":24.953769177454625}]
["ANAMET-M",2691993,"95 mm","Fittings for gigant conduit, Straight fixed with flange, IP 54",1,30.518664090818483,{"$f":"F2728*(1-Elteq!$F$5)","v":30.518664090818483}]
["ANAMET-M",2692703,"70 mm","Fittings for gigant conduit, 90° elbow fixed with flange, IP 54",1,32.627564166500605,{"$f":"F2729*(1-Elteq!$F$5)","v":32.627564166500605}]
["ANAMET-M",2692993,"95 mm","Fittings for gigant conduit, 90° elbow fixed with flange, IP 54",1,42.493872009559738,{"$f":"F2730*(1-Elteq!$F$5)","v":42.493872009559738}]
["ANAMET-M",2693703,"70 mm","Fittings for gigant conduit, 90° elbow fixed with flange, IP 54",1,32.627564166500605,{"$f":"F2731*(1-Elteq!$F$5)","v":32.627564166500605}]
["ANAMET-M",2693993,"95 mm","Fittings for gigant conduit, 90° elbow fixed with flange, IP 54",1,42.493872009559738,{"$f":"F2732*(1-Elteq!$F$5)","v":42.493872009559738}]
["ANAMET-M",8100111,"PG 11","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",1,4.8867023780123349,{"$f":"F2733*(1-Elteq!$F$5)","v":4.8867023780123349}]
["ANAMET-M",8100161,"PG 16","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",1,5.7042495439155392,{"$f":"F2734*(1-Elteq!$F$5)","v":5.7042495439155392}]
["ANAMET-M",8100211,"PG 21","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",1,7.5530209759011955,{"$f":"F2735*(1-Elteq!$F$5)","v":7.5530209759011955}]
["ANAMET-M",8100291,"PG 29","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",1,13.006432184823705,{"$f":"F2736*(1-Elteq!$F$5)","v":13.006432184823705}]
["ANAMET-M",8100361,"PG 36","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",1,21.414161561441887,{"$f":"F2737*(1-Elteq!$F$5)","v":21.414161561441887}]
["ANAMET-M",8100421,"PG 42","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",1,28.734924819756944,{"$f":"F2738*(1-Elteq!$F$5)","v":28.734924819756944}]
["ANAMET-M",8100481,"PG 48","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",1,44.063934180442025,{"$f":"F2739*(1-Elteq!$F$5)","v":44.063934180442025}]
["ANAMET-M",8120161,"M16 x 1,5","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",1,4.5801221907986331,{"$f":"F2740*(1-Elteq!$F$5)","v":4.5801221907986331}]
["ANAMET-M",8120171,"M20 x 1,5","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",1,4.9238636128261177,{"$f":"F2741*(1-Elteq!$F$5)","v":4.9238636128261177}]
["ANAMET-M",8120201,"M20 x 1,5","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",1,4.9238636128261177,{"$f":"F2742*(1-Elteq!$F$5)","v":4.9238636128261177}]
["ANAMET-M",8120251,"M25 x 1,5","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",1,7.2650214060943847,{"$f":"F2743*(1-Elteq!$F$5)","v":7.2650214060943847}]
["ANAMET-M",8120321,"M32 x 1,5","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",1,11.61288587930688,{"$f":"F2744*(1-Elteq!$F$5)","v":11.61288587930688}]
["ANAMET-M",8120401,"M40 x 1,5","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",1,21.414161561441887,{"$f":"F2745*(1-Elteq!$F$5)","v":21.414161561441887}]
["ANAMET-M",8120501,"M50 x 1,5","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",1,28.734924819756944,{"$f":"F2746*(1-Elteq!$F$5)","v":28.734924819756944}]
["ANAMET-M",8120631,"M63 x 1,5","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",1,44.063934180442025,{"$f":"F2747*(1-Elteq!$F$5)","v":44.063934180442025}]
["ANAMET-M",8175120,"13 mm","Fittings for Hiprojacket, Clamping ring for mounting fittings",1,2.0067066799442288,{"$f":"F2748*(1-Elteq!$F$5)","v":2.0067066799442288}]
["ANAMET-M",8175160,"16 mm","Fittings for Hiprojacket, Clamping ring for mounting fittings",1,2.5641252021509588,{"$f":"F2749*(1-Elteq!$F$5)","v":2.5641252021509588}]
["ANAMET-M",8175200,"22 mm","Fittings for Hiprojacket, Clamping ring for mounting fittings",1,3.0658018721370164,{"$f":"F2750*(1-Elteq!$F$5)","v":3.0658018721370164}]
["ANAMET-M",8175260,"25 mm","Fittings for Hiprojacket, Clamping ring for mounting fittings",1,4.0691552121091306,{"$f":"F2751*(1-Elteq!$F$5)","v":4.0691552121091306}]
["ANAMET-M",8175350,"35 mm","Fittings for Hiprojacket, Clamping ring for mounting fittings",1,4.738057438757207,{"$f":"F2752*(1-Elteq!$F$5)","v":4.738057438757207}]
["ANAMET-M",8175400,"38 mm","Fittings for Hiprojacket, Clamping ring for mounting fittings",1,8.1383104242182611,{"$f":"F2753*(1-Elteq!$F$5)","v":8.1383104242182611}]
["ANAMET-M",8175500,"51 mm","Fittings for Hiprojacket, Clamping ring for mounting fittings",1,14.938816395140369,{"$f":"F2754*(1-Elteq!$F$5)","v":14.938816395140369}]
["ANAMET-M",8100111,"PG 11","Fittings for Thermojacket S, Clamping ring for mounting fittings",1,4.8867023780123349,{"$f":"F2755*(1-Elteq!$F$5)","v":4.8867023780123349}]
["ANAMET-M",8100161,"PG 16","Fittings for Thermojacket S, Clamping ring for mounting fittings",1,5.7042495439155392,{"$f":"F2756*(1-Elteq!$F$5)","v":5.7042495439155392}]
["ANAMET-M",8100211,"PG 21","Fittings for Thermojacket S, Clamping ring for mounting fittings",1,7.5530209759011955,{"$f":"F2757*(1-Elteq!$F$5)","v":7.5530209759011955}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-M"},8100291,"PG 29","Fittings for Thermojacket S, Clamping ring for mounting fittings",1,13.006432184823705,{"$f":"F2758*(1-Elteq!$F$5)","v":13.006432184823705}]
["ANAMET-M",8100361,"PG 36","Fittings for Thermojacket S, Clamping ring for mounting fittings",1,21.414161561441887,{"$f":"F2759*(1-Elteq!$F$5)","v":21.414161561441887}]
["ANAMET-M",8100421,"PG 42","Fittings for Thermojacket S, Clamping ring for mounting fittings",1,28.734924819756944,{"$f":"F2760*(1-Elteq!$F$5)","v":28.734924819756944}]
["ANAMET-M",8100481,"PG 48","Fittings for Thermojacket S, Clamping ring for mounting fittings",1,44.063934180442025,{"$f":"F2761*(1-Elteq!$F$5)","v":44.063934180442025}]
["ANAMET-M",8120161,"M16 x 1,5","Fittings for Thermojacket S, Clamping ring for mounting fittings",1,4.5801221907986331,{"$f":"F2762*(1-Elteq!$F$5)","v":4.5801221907986331}]
["ANAMET-M",8120171,"M20 x 1,5","Fittings for Thermojacket S, Clamping ring for mounting fittings",1,4.9238636128261177,{"$f":"F2763*(1-Elteq!$F$5)","v":4.9238636128261177}]
["ANAMET-M",8120201,"M20 x 1,5","Fittings for Thermojacket S, Clamping ring for mounting fittings",1,4.9238636128261177,{"$f":"F2764*(1-Elteq!$F$5)","v":4.9238636128261177}]
["ANAMET-M",8120251,"M25 x 1,5","Fittings for Thermojacket S, Clamping ring for mounting fittings",1,7.2650214060943847,{"$f":"F2765*(1-Elteq!$F$5)","v":7.2650214060943847}]
["ANAMET-M",8120321,"M32 x 1,5","Fittings for Thermojacket S, Clamping ring for mounting fittings",1,11.61288587930688,{"$f":"F2766*(1-Elteq!$F$5)","v":11.61288587930688}]
["ANAMET-M",8120401,"M40 x 1,5","Fittings for Thermojacket S, Clamping ring for mounting fittings",1,21.414161561441887,{"$f":"F2767*(1-Elteq!$F$5)","v":21.414161561441887}]
["ANAMET-M",8120501,"M50 x 1,5","Fittings for Thermojacket S, Clamping ring for mounting fittings",1,28.734924819756944,{"$f":"F2768*(1-Elteq!$F$5)","v":28.734924819756944}]
["ANAMET-M",8120631,"M63 x 1,5","Fittings for Thermojacket S, Clamping ring for mounting fittings",1,44.063934180442025,{"$f":"F2769*(1-Elteq!$F$5)","v":44.063934180442025}]
["ANAMET-M",8176120,"TJ- 10","Fittings for Thermojacket S, Clamping ring for mounting fittings",1,2.0067066799442288,{"$f":"F2770*(1-Elteq!$F$5)","v":2.0067066799442288}]
["ANAMET-M",8176160,"TJ- 10","Fittings for Thermojacket S, Clamping ring for mounting fittings",1,2.5641252021509588,{"$f":"F2771*(1-Elteq!$F$5)","v":2.5641252021509588}]
["ANAMET-M",8176200,"TJ- 14","Fittings for Thermojacket S, Clamping ring for mounting fittings",1,3.0658018721370164,{"$f":"F2772*(1-Elteq!$F$5)","v":3.0658018721370164}]
["ANAMET-M",8176260,"TJ- 14","Fittings for Thermojacket S, Clamping ring for mounting fittings",1,4.0691552121091306,{"$f":"F2773*(1-Elteq!$F$5)","v":4.0691552121091306}]
["ANAMET-M",8176350,"TJ- 22","Fittings for Thermojacket S, Clamping ring for mounting fittings",1,4.738057438757207,{"$f":"F2774*(1-Elteq!$F$5)","v":4.738057438757207}]
["ANAMET-M",8176400,"TJ- 22","Fittings for Thermojacket S, Clamping ring for mounting fittings",1,8.1383104242182611,{"$f":"F2775*(1-Elteq!$F$5)","v":8.1383104242182611}]
["ANAMET-M",8176500,"TJ- 44","Fittings for Thermojacket S, Clamping ring for mounting fittings",1,14.938816395140369,{"$f":"F2776*(1-Elteq!$F$5)","v":14.938816395140369}]

{"sheet":"ANAMET-S","index":3,"n_rows":4103,"n_cols":7,"rows_kept":4103,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["sheetname","Objednávací kód","Rozmer","Popis","Počet ks alebo m (štandardné balenie)","Cena za ks alebo m (štandardné balenie)","Cena po zľave za ks alebo m \n(štandardné balenie)"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},2560120,"M12 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",10,1.9881260625373383,{"$f":"F5*(1-Elteq!$F$6)","v":1.9881260625373383}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},2560150,"M16 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",10,1.9881260625373383,{"$f":"F6*(1-Elteq!$F$6)","v":1.9881260625373383}]
["ANAMET-S",2560160,"M16 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",10,2.2761256323441486,{"$f":"F7*(1-Elteq!$F$6)","v":2.2761256323441486}]
["ANAMET-S",2560170,"M20 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",10,2.4805124238199494,{"$f":"F8*(1-Elteq!$F$6)","v":2.4805124238199494}]
["ANAMET-S",2560200,"M20 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",10,2.9636084763991155,{"$f":"F9*(1-Elteq!$F$6)","v":2.9636084763991155}]
["ANAMET-S",2560250,"M25 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",5,4.3107032383987134,{"$f":"F10*(1-Elteq!$F$6)","v":4.3107032383987134}]
["ANAMET-S",2560320,"M32 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",5,7.5065694323839676,{"$f":"F11*(1-Elteq!$F$6)","v":7.5065694323839676}]
["ANAMET-S",2560400,"M40 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",2,12.616239219278995,{"$f":"F12*(1-Elteq!$F$6)","v":12.616239219278995}]
["ANAMET-S",2560500,"M50 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",2,22.064483170683072,{"$f":"F13*(1-Elteq!$F$6)","v":22.064483170683072}]
["ANAMET-S",2560600,"M63 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",2,31.56846897430782,{"$f":"F14*(1-Elteq!$F$6)","v":31.56846897430782}]
["ANAMET-S",2561120,"M12 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",10,2.5548348934475134,{"$f":"F15*(1-Elteq!$F$6)","v":2.5548348934475134}]
["ANAMET-S",2561150,"M16 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",10,2.6756089065923048,{"$f":"F16*(1-Elteq!$F$6)","v":2.6756089065923048}]
["ANAMET-S",2561160,"M16 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",10,2.6848992152957507,{"$f":"F17*(1-Elteq!$F$6)","v":2.6848992152957507}]
["ANAMET-S",2561170,"M20 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",10,3.0565115634335709,{"$f":"F18*(1-Elteq!$F$6)","v":3.0565115634335709}]
["ANAMET-S",2561200,"M20 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",10,3.6789622465644194,{"$f":"F19*(1-Elteq!$F$6)","v":3.6789622465644194}]
["ANAMET-S",2561250,"M25 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",5,5.5184433698466293,{"$f":"F20*(1-Elteq!$F$6)","v":5.5184433698466293}]
["ANAMET-S",2561320,"M32 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",5,9.7641144473212247,{"$f":"F21*(1-Elteq!$F$6)","v":9.7641144473212247}]
["ANAMET-S",2561400,"M40 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",2,16.40668517028476,{"$f":"F22*(1-Elteq!$F$6)","v":16.40668517028476}]
["ANAMET-S",2561500,"M50 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",2,37.309879753037144,{"$f":"F23*(1-Elteq!$F$6)","v":37.309879753037144}]
["ANAMET-S",2561600,"M63 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",2,41.044583851822239,{"$f":"F24*(1-Elteq!$F$6)","v":41.044583851822239}]
["ANAMET-S",3700122,"10 mm","FCEN conduit without cover, Galvanised steel, IP 40",25,2.2575450149372576,{"$f":"F25*(1-Elteq!$F$6)","v":2.2575450149372576}]
["ANAMET-S",3700125,"10 mm","FCEN conduit without cover, Galvanised steel, IP 40",50,2.1553516191993567,{"$f":"F26*(1-Elteq!$F$6)","v":2.1553516191993567}]
["ANAMET-S",3700161,"13 mm","FCEN conduit without cover, Galvanised steel, IP 40",10,2.9171569328818885,{"$f":"F27*(1-Elteq!$F$6)","v":2.9171569328818885}]
["ANAMET-S",3700162,"13 mm","FCEN conduit without cover, Galvanised steel, IP 40",25,2.7127701414060872,{"$f":"F28*(1-Elteq!$F$6)","v":2.7127701414060872}]
["ANAMET-S",3700165,"13 mm","FCEN conduit without cover, Galvanised steel, IP 40",50,2.5734155108544043,{"$f":"F29*(1-Elteq!$F$6)","v":2.5734155108544043}]
["ANAMET-S",3700201,"16,9 mm","FCEN conduit without cover, Galvanised steel, IP 40",10,3.5117366899024001,{"$f":"F30*(1-Elteq!$F$6)","v":3.5117366899024001}]
["ANAMET-S",3700202,"16,9 mm","FCEN conduit without cover, Galvanised steel, IP 40",25,3.2701886636128177,{"$f":"F31*(1-Elteq!$F$6)","v":3.2701886636128177}]
["ANAMET-S",3700205,"16,9 mm","FCEN conduit without cover, Galvanised steel, IP 40",50,3.1308340330611348,{"$f":"F32*(1-Elteq!$F$6)","v":3.1308340330611348}]
["ANAMET-S",3700251,"21,2 mm","FCEN conduit without cover, Galvanised steel, IP 40",10,5.0910891694881366,{"$f":"F33*(1-Elteq!$F$6)","v":5.0910891694881366}]
["ANAMET-S",3700252,"21,2 mm","FCEN conduit without cover, Galvanised steel, IP 40",25,4.4965094124676241,{"$f":"F34*(1-Elteq!$F$6)","v":4.4965094124676241}]
["ANAMET-S",3700255,"21,2 mm","FCEN conduit without cover, Galvanised steel, IP 40",50,4.0970261382194675,{"$f":"F35*(1-Elteq!$F$6)","v":4.0970261382194675}]
["ANAMET-S",3700321,"28 mm","FCEN conduit without cover, Galvanised steel, IP 40",10,6.8748284405496731,{"$f":"F36*(1-Elteq!$F$6)","v":6.8748284405496731}]
["ANAMET-S",3700322,"28 mm","FCEN conduit without cover, Galvanised steel, IP 40",25,5.6206367655845302,{"$f":"F37*(1-Elteq!$F$6)","v":5.6206367655845302}]
["ANAMET-S",3700401,"37,7 mm","FCEN conduit without cover, Galvanised steel, IP 40",10,10.052114017128035,{"$f":"F38*(1-Elteq!$F$6)","v":10.052114017128035}]
["ANAMET-S",3700402,"37,7 mm","FCEN conduit without cover, Galvanised steel, IP 40",25,9.40179240788685,{"$f":"F39*(1-Elteq!$F$6)","v":9.40179240788685}]
["ANAMET-S",3700501,"48,4 mm","FCEN conduit without cover, Galvanised steel, IP 40",10,14.56720404700255,{"$f":"F40*(1-Elteq!$F$6)","v":14.56720404700255}]
["ANAMET-S",3700502,"48,4 mm","FCEN conduit without cover, Galvanised steel, IP 40",25,13.647463485361445,{"$f":"F41*(1-Elteq!$F$6)","v":13.647463485361445}]
["ANAMET-S",2641120,"-","Multiflex fittings for FCEN, End cap, IP 40",10,1.2727722923720342,{"$f":"F42*(1-Elteq!$F$6)","v":1.2727722923720342}]
["ANAMET-S",2641160,"-","Multiflex fittings for FCEN, End cap, IP 40",10,1.5886427882891812,{"$f":"F43*(1-Elteq!$F$6)","v":1.5886427882891812}]
["ANAMET-S",2641200,"-","Multiflex fittings for FCEN, End cap, IP 40",10,1.969545445130447,{"$f":"F44*(1-Elteq!$F$6)","v":1.969545445130447}]
["ANAMET-S",2641250,"-","Multiflex fittings for FCEN, End cap, IP 40",5,2.7406410675164237,{"$f":"F45*(1-Elteq!$F$6)","v":2.7406410675164237}]
["ANAMET-S",2641320,"-","Multiflex fittings for FCEN, End cap, IP 40",5,4.0784455208125756,{"$f":"F46*(1-Elteq!$F$6)","v":4.0784455208125756}]
["ANAMET-S",2641400,"-","Multiflex fittings for FCEN, End cap, IP 40",2,7.8317302370045585,{"$f":"F47*(1-Elteq!$F$6)","v":7.8317302370045585}]
["ANAMET-S",2641500,"-","Multiflex fittings for FCEN, End cap, IP 40",2,12.095981931886046,{"$f":"F48*(1-Elteq!$F$6)","v":12.095981931886046}]
["ANAMET-S",7120143,"M20 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",10,4.7194768213503169,{"$f":"F49*(1-Elteq!$F$6)","v":4.7194768213503169}]
["ANAMET-S",7120153,"M16 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",10,4.4686384863572872,{"$f":"F50*(1-Elteq!$F$6)","v":4.4686384863572872}]
["ANAMET-S",7120163,"M16 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",10,3.6325107030471919,{"$f":"F51*(1-Elteq!$F$6)","v":3.6325107030471919}]
["ANAMET-S",7120173,"M20 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",10,3.8833490380402202,{"$f":"F52*(1-Elteq!$F$6)","v":3.8833490380402202}]
["ANAMET-S",7120203,"M20 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",10,4.1527679904401413,{"$f":"F53*(1-Elteq!$F$6)","v":4.1527679904401413}]
["ANAMET-S",7120253,"M25 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",5,6.1594746703843688,{"$f":"F54*(1-Elteq!$F$6)","v":6.1594746703843688}]
["ANAMET-S",7120323,"M32 x 1,5","Multiflex fittings for FCEN, Straight fixed with male thread, IP 40",5,10.284371734714174,{"$f":"F55*(1-Elteq!$F$6)","v":10.284371734714174}]
["ANAMET-S",8127153,"M16 x 1,5","Multiflex fittings for FCEN, Straight cablehose male thread, IP 68",10,10.76746778729334,{"$f":"F56*(1-Elteq!$F$6)","v":10.76746778729334}]
["ANAMET-S",8127163,"M16 x 1,5","Multiflex fittings for FCEN, Straight cablehose male thread, IP 68",10,12.820626010754795,{"$f":"F57*(1-Elteq!$F$6)","v":12.820626010754795}]
["ANAMET-S",8127173,"M20 x 1,5","Multiflex fittings for FCEN, Straight cablehose male thread, IP 68",10,10.860370874327794,{"$f":"F58*(1-Elteq!$F$6)","v":10.860370874327794}]
["ANAMET-S",8127203,"M20 x 1,5","Multiflex fittings for FCEN, Straight cablehose male thread, IP 68",10,14.660107134037005,{"$f":"F59*(1-Elteq!$F$6)","v":14.660107134037005}]
["ANAMET-S",8127253,"M25 x 1,5","Multiflex fittings for FCEN, Straight cablehose male thread, IP 68",5,20.466550073690449,{"$f":"F60*(1-Elteq!$F$6)","v":20.466550073690449}]
["ANAMET-S",8127323,"M32 x 1,5","Multiflex fittings for FCEN, Straight cablehose male thread, IP 68",5,51.561213304122553,{"$f":"F61*(1-Elteq!$F$6)","v":51.561213304122553}]
["ANAMET-S",8130153,"M16 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",10,7.9246333240390161,{"$f":"F62*(1-Elteq!$F$6)","v":7.9246333240390161}]
["ANAMET-S",8130163,"M16 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",10,7.3950857279426208,{"$f":"F63*(1-Elteq!$F$6)","v":7.3950857279426208}]
["ANAMET-S",8130203,"M20 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",10,8.3798584505078431,{"$f":"F64*(1-Elteq!$F$6)","v":8.3798584505078431}]
["ANAMET-S",8130253,"M25 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",5,10.971854578769141,{"$f":"F65*(1-Elteq!$F$6)","v":10.971854578769141}]
["ANAMET-S",8130323,"M32 x 1,5","Multiflex fittings for FCEN, Straight swivel with male thread, IP 40",5,18.645649567815127,{"$f":"F66*(1-Elteq!$F$6)","v":18.645649567815127}]
["ANAMET-S",8171120,"-","Multiflex fittings for FCEN, Connection set for FCEN",10,0.74322469627564036,{"$f":"F67*(1-Elteq!$F$6)","v":0.74322469627564036}]
["ANAMET-S",8171160,"-","Multiflex fittings for FCEN, Connection set for FCEN",10,0.83612778331009541,{"$f":"F68*(1-Elteq!$F$6)","v":0.83612778331009541}]
["ANAMET-S",8171200,"-","Multiflex fittings for FCEN, Connection set for FCEN",10,0.92903087034455045,{"$f":"F69*(1-Elteq!$F$6)","v":0.92903087034455045}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8171250,"-","Multiflex fittings for FCEN, Connection set for FCEN",5,1.161288587930688,{"$f":"F70*(1-Elteq!$F$6)","v":1.161288587930688}]
["ANAMET-S",8171320,"-","Multiflex fittings for FCEN, Connection set for FCEN",5,2.322577175861376,{"$f":"F71*(1-Elteq!$F$6)","v":2.322577175861376}]
["ANAMET-S",1070102,"5/16\"","SL conduit without cover, Galvanised steel, IP 40",30,2.3318674845648215,{"$f":"F72*(1-Elteq!$F$6)","v":2.3318674845648215}]
["ANAMET-S",1070122,"3/8\"","SL conduit without cover, Galvanised steel, IP 40",30,2.7963829197370966,{"$f":"F73*(1-Elteq!$F$6)","v":2.7963829197370966}]
["ANAMET-S",1070162,"1/2\"","SL conduit without cover, Galvanised steel, IP 40",30,3.1679952678749173,{"$f":"F74*(1-Elteq!$F$6)","v":3.1679952678749173}]
["ANAMET-S",1070202,"3/4\"","SL conduit without cover, Galvanised steel, IP 40",30,4.3571547819159422,{"$f":"F75*(1-Elteq!$F$6)","v":4.3571547819159422}]
["ANAMET-S",1070262,"1\"","SL conduit without cover, Galvanised steel, IP 40",30,6.6704416490738714,{"$f":"F76*(1-Elteq!$F$6)","v":6.6704416490738714}]
["ANAMET-S",1070352,"1.1/4\"","SL conduit without cover, Galvanised steel, IP 40",30,9.9592109300935814,{"$f":"F77*(1-Elteq!$F$6)","v":9.9592109300935814}]
["ANAMET-S",6000102,"5/16\"","SLI conduit without cover, Stainless steel AISI-304, IP 40",30,7.00489276239791,{"$f":"F78*(1-Elteq!$F$6)","v":7.00489276239791}]
["ANAMET-S",6000122,"3/8\"","SLI conduit without cover, Stainless steel AISI-304, IP 40",30,8.0732782632941422,{"$f":"F79*(1-Elteq!$F$6)","v":8.0732782632941422}]
["ANAMET-S",6000162,"1/2\"","SLI conduit without cover, Stainless steel AISI-304, IP 40",30,8.4356003027285169,{"$f":"F80*(1-Elteq!$F$6)","v":8.4356003027285169}]
["ANAMET-S",6000202,"3/4\"","SLI conduit without cover, Stainless steel AISI-304, IP 40",30,10.776758095996785,{"$f":"F81*(1-Elteq!$F$6)","v":10.776758095996785}]
["ANAMET-S",6000262,"1\"","SLI conduit without cover, Stainless steel AISI-304, IP 40",30,15.682041091416011,{"$f":"F82*(1-Elteq!$F$6)","v":15.682041091416011}]
["ANAMET-S",6000352,"1 1/4\"","SLI conduit without cover, Stainless steel AISI-304, IP 40",30,21.070420139414406,{"$f":"F83*(1-Elteq!$F$6)","v":21.070420139414406}]
["ANAMET-S",6006102,"5/16\"","SLI-316 conduit without cover, Stainless steel AISI-316, IP 40",30,9.1416637641903744,{"$f":"F84*(1-Elteq!$F$6)","v":9.1416637641903744}]
["ANAMET-S",6006122,"3/8\"","SLI-316 conduit without cover, Stainless steel AISI-316, IP 40",30,11.194821987651833,{"$f":"F85*(1-Elteq!$F$6)","v":11.194821987651833}]
["ANAMET-S",6006162,"1/2\"","SLI-316 conduit without cover, Stainless steel AISI-316, IP 40",30,12.58836829316866,{"$f":"F86*(1-Elteq!$F$6)","v":12.58836829316866}]
["ANAMET-S",6006202,"3/4\"","SLI-316 conduit without cover, Stainless steel AISI-316, IP 40",30,16.964103692491491,{"$f":"F87*(1-Elteq!$F$6)","v":16.964103692491491}]
["ANAMET-S",6006262,"1\"","SLI-316 conduit without cover, Stainless steel AISI-316, IP 40",30,23.327965154351659,{"$f":"F88*(1-Elteq!$F$6)","v":23.327965154351659}]
["ANAMET-S",6006352,"1 1/4\"","SLI-316 conduit without cover, Stainless steel AISI-316, IP 40",30,32.17233904003178,{"$f":"F89*(1-Elteq!$F$6)","v":32.17233904003178}]
["ANAMET-S",7100116,"PG 11","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",10,3.6789622465644194,{"$f":"F90*(1-Elteq!$F$6)","v":3.6789622465644194}]
["ANAMET-S",7100136,"PG 13,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",10,3.6882525552678653,{"$f":"F91*(1-Elteq!$F$6)","v":3.6882525552678653}]
["ANAMET-S",7100166,"PG 16","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",10,4.2921226209918233,{"$f":"F92*(1-Elteq!$F$6)","v":4.2921226209918233}]
["ANAMET-S",7100216,"PG 21","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",5,6.2616680661222697,{"$f":"F93*(1-Elteq!$F$6)","v":6.2616680661222697}]
["ANAMET-S",7100296,"PG 29","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",5,10.628113156741655,{"$f":"F94*(1-Elteq!$F$6)","v":10.628113156741655}]
["ANAMET-S",7100366,"PG 36","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",2,16.490297948615769,{"$f":"F95*(1-Elteq!$F$6)","v":16.490297948615769}]
["ANAMET-S",7120146,"M20 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",10,3.9762521250746765,{"$f":"F96*(1-Elteq!$F$6)","v":3.9762521250746765}]
["ANAMET-S",7120156,"M16 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",10,3.7254137900816469,{"$f":"F97*(1-Elteq!$F$6)","v":3.7254137900816469}]
["ANAMET-S",7120166,"M16 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",10,3.6325107030471924,{"$f":"F98*(1-Elteq!$F$6)","v":3.6325107030471924}]
["ANAMET-S",7120176,"M20 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",10,3.8833490380402202,{"$f":"F99*(1-Elteq!$F$6)","v":3.8833490380402202}]
["ANAMET-S",7120206,"M20 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",10,4.1527679904401404,{"$f":"F100*(1-Elteq!$F$6)","v":4.1527679904401404}]
["ANAMET-S",7120256,"M25 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",5,6.1594746703843688,{"$f":"F101*(1-Elteq!$F$6)","v":6.1594746703843688}]
["ANAMET-S",7120326,"M32 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",5,10.284371734714174,{"$f":"F102*(1-Elteq!$F$6)","v":10.284371734714174}]
["ANAMET-S",7120406,"M40 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",2,16.369523935470976,{"$f":"F103*(1-Elteq!$F$6)","v":16.369523935470976}]
["ANAMET-S",7129146,"M20 x 1,5","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",10,7.5808919020115315,{"$f":"F104*(1-Elteq!$F$6)","v":7.5808919020115315}]
["ANAMET-S",7129156,"M16 x 1,5","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",10,6.0294103485361328,{"$f":"F105*(1-Elteq!$F$6)","v":6.0294103485361328}]
["ANAMET-S",7129166,"M16 x 1,5","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",10,5.862184791874113,{"$f":"F106*(1-Elteq!$F$6)","v":5.862184791874113}]
["ANAMET-S",7129176,"M20 x 1,5","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",10,6.7447641187014371,{"$f":"F107*(1-Elteq!$F$6)","v":6.7447641187014371}]
["ANAMET-S",7129206,"M20 x 1,5","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",10,6.921279984066901,{"$f":"F108*(1-Elteq!$F$6)","v":6.921279984066901}]
["ANAMET-S",7129256,"M25 x 1,5","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",5,10.637403465445102,{"$f":"F109*(1-Elteq!$F$6)","v":10.637403465445102}]
["ANAMET-S",7129326,"M32 x 1,5","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",5,19.574680438159678,{"$f":"F110*(1-Elteq!$F$6)","v":19.574680438159678}]
["ANAMET-S",7129406,"M40 x 1,5","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",2,31.215437243576893,{"$f":"F111*(1-Elteq!$F$6)","v":31.215437243576893}]
["ANAMET-S",8130156,"M16 x 1,5","Multiflex fittings for SL / SLI, Straight swivel with male thread, IP 40",10,7.9246333240390143,{"$f":"F112*(1-Elteq!$F$6)","v":7.9246333240390143}]
["ANAMET-S",8130166,"M16 x 1,5","Multiflex fittings for SL / SLI, Straight swivel with male thread, IP 40",10,7.3950857279426208,{"$f":"F113*(1-Elteq!$F$6)","v":7.3950857279426208}]
["ANAMET-S",8130206,"M20 x 1,5","Multiflex fittings for SL / SLI, Straight swivel with male thread, IP 40",10,8.3798584505078431,{"$f":"F114*(1-Elteq!$F$6)","v":8.3798584505078431}]
["ANAMET-S",8130256,"M25 x 1,5","Multiflex fittings for SL / SLI, Straight swivel with male thread, IP 40",5,14.687978060147342,{"$f":"F115*(1-Elteq!$F$6)","v":14.687978060147342}]
["ANAMET-S",8130326,"M32 x 1,5","Multiflex fittings for SL / SLI, Straight swivel with male thread, IP 40",5,18.645649567815127,{"$f":"F116*(1-Elteq!$F$6)","v":18.645649567815127}]
["ANAMET-S",8130406,"M40 x 1,5","Multiflex fittings for SL / SLI, Straight swivel with male thread, IP 40",2,22.380353666600222,{"$f":"F117*(1-Elteq!$F$6)","v":22.380353666600222}]
["ANAMET-S",8139156,"M16 x 1,5","Multiflex fittings for SL / SLI, 90° elbow swivel with male thread, IP 40",10,13.80539873332002,{"$f":"F118*(1-Elteq!$F$6)","v":13.80539873332002}]
["ANAMET-S",8139166,"M16 x 1,5","Multiflex fittings for SL / SLI, 90° elbow swivel with male thread, IP 40",10,12.356110575582521,{"$f":"F119*(1-Elteq!$F$6)","v":12.356110575582521}]
["ANAMET-S",8139206,"M20 x 1,5","Multiflex fittings for SL / SLI, 90° elbow swivel with male thread, IP 40",10,15.849266648078029,{"$f":"F120*(1-Elteq!$F$6)","v":15.849266648078029}]
["ANAMET-S",8139256,"M20 x 1,5","Multiflex fittings for SL / SLI, 90° elbow swivel with male thread, IP 40",5,25.120994734116643,{"$f":"F121*(1-Elteq!$F$6)","v":25.120994734116643}]
["ANAMET-S",8139326,"M25 x 1,5","Multiflex fittings for SL / SLI, 90° elbow swivel with male thread, IP 40",5,40.895938912567111,{"$f":"F122*(1-Elteq!$F$6)","v":40.895938912567111}]
["ANAMET-S",8172106,"M32 x 1,5","Multiflex fittings for SL / SLI, Connection ring SL / SLI",10,0.74322469627564036,{"$f":"F123*(1-Elteq!$F$6)","v":0.74322469627564036}]
["ANAMET-S",8172136,"-","Multiflex fittings for SL / SLI, Connection ring SL / SLI",10,0.83612778331009541,{"$f":"F124*(1-Elteq!$F$6)","v":0.83612778331009541}]
["ANAMET-S",8172166,"-","Multiflex fittings for SL / SLI, Connection ring SL / SLI",10,0.92903087034455045,{"$f":"F125*(1-Elteq!$F$6)","v":0.92903087034455045}]
["ANAMET-S",8172206,"-","Multiflex fittings for SL / SLI, Connection ring SL / SLI",5,1.161288587930688,{"$f":"F126*(1-Elteq!$F$6)","v":1.161288587930688}]
["ANAMET-S",8172266,"-","Multiflex fittings for SL / SLI, Connection ring SL / SLI",5,2.322577175861376,{"$f":"F127*(1-Elteq!$F$6)","v":2.322577175861376}]
["ANAMET-S",8172356,"-","Multiflex fittings for SL / SLI, Connection ring SL / SLI",2,3.5303173073092915,{"$f":"F128*(1-Elteq!$F$6)","v":3.5303173073092915}]
["ANAMET-S",7109116,"PG 11","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",10,6.0665715833499139,{"$f":"F129*(1-Elteq!$F$6)","v":6.0665715833499139}]
["ANAMET-S",7109136,"PG 13,5","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",10,6.2337971400119327,{"$f":"F130*(1-Elteq!$F$6)","v":6.2337971400119327}]
["ANAMET-S",7109166,"PG 16","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",10,7.3207632583150577,{"$f":"F131*(1-Elteq!$F$6)","v":7.3207632583150577}]
["ANAMET-S",7109216,"PG 21","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",5,10.525919761003756,{"$f":"F132*(1-Elteq!$F$6)","v":10.525919761003756}]
["ANAMET-S",7109296,"PG 29","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",5,19.816228464449257,{"$f":"F133*(1-Elteq!$F$6)","v":19.816228464449257}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},7109366,"PG 36","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",2,31.215437243576893,{"$f":"F134*(1-Elteq!$F$6)","v":31.215437243576893}]
["ANAMET-S",7140126,"NPT 1/2\"","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",10,3.7811556423023203,{"$f":"F135*(1-Elteq!$F$6)","v":3.7811556423023203}]
["ANAMET-S",7140166,"NPT 1/2\"","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",10,4.3014129296952683,{"$f":"F136*(1-Elteq!$F$6)","v":4.3014129296952683}]
["ANAMET-S",7140206,"NPT 3/4\"","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",5,5.890055717984449,{"$f":"F137*(1-Elteq!$F$6)","v":5.890055717984449}]
["ANAMET-S",7140266,"NPT 1\"","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",5,10.637403465445102,{"$f":"F138*(1-Elteq!$F$6)","v":10.637403465445102}]
["ANAMET-S",7140356,"NPT 1.1/4\"","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",2,17.057006779525945,{"$f":"F139*(1-Elteq!$F$6)","v":17.057006779525945}]
["ANAMET-S",7149126,"NPT 1/2\"","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",10,6.3081196096394976,{"$f":"F140*(1-Elteq!$F$6)","v":6.3081196096394976}]
["ANAMET-S",7149166,"NPT 1/2\"","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",10,7.4415372714598487,{"$f":"F141*(1-Elteq!$F$6)","v":7.4415372714598487}]
["ANAMET-S",7149206,"NPT 3/4\"","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",5,10.470177908783082,{"$f":"F142*(1-Elteq!$F$6)","v":10.470177908783082}]
["ANAMET-S",7149266,"NPT 1\"","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",5,19.574680438159678,{"$f":"F143*(1-Elteq!$F$6)","v":19.574680438159678}]
["ANAMET-S",7149356,"NPT 1.1/4\"","Multiflex fittings for SL / SLI, 90° elbow fixed with male thread, IP 40",2,31.215437243576893,{"$f":"F144*(1-Elteq!$F$6)","v":31.215437243576893}]
["ANAMET-S",7840106,"-","Multiflex fittings for SL / SLI, Conduit connector, IP 40",10,6.921279984066901,{"$f":"F145*(1-Elteq!$F$6)","v":6.921279984066901}]
["ANAMET-S",7840126,"-","Multiflex fittings for SL / SLI, Conduit connector, IP 40",10,5.9922491137223508,{"$f":"F146*(1-Elteq!$F$6)","v":5.9922491137223508}]
["ANAMET-S",7840166,"-","Multiflex fittings for SL / SLI, Conduit connector, IP 40",10,7.1999892451702658,{"$f":"F147*(1-Elteq!$F$6)","v":7.1999892451702658}]
["ANAMET-S",7840206,"-","Multiflex fittings for SL / SLI, Conduit connector, IP 40",5,10.590951921927875,{"$f":"F148*(1-Elteq!$F$6)","v":10.590951921927875}]
["ANAMET-S",7840266,"-","Multiflex fittings for SL / SLI, Conduit connector, IP 40",5,19.240229324835639,{"$f":"F149*(1-Elteq!$F$6)","v":19.240229324835639}]
["ANAMET-S",7840356,"-","Multiflex fittings for SL / SLI, Conduit connector, IP 40",2,26.22654146982666,{"$f":"F150*(1-Elteq!$F$6)","v":26.22654146982666}]
["ANAMET-S",8100096,"PG 9","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",10,5.1096697868950267,{"$f":"F151*(1-Elteq!$F$6)","v":5.1096697868950267}]
["ANAMET-S",8100106,"PG 9","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",10,6.958441218880683,{"$f":"F152*(1-Elteq!$F$6)","v":6.958441218880683}]
["ANAMET-S",8100116,"PG 11","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",10,7.079215232025474,{"$f":"F153*(1-Elteq!$F$6)","v":7.079215232025474}]
["ANAMET-S",8100126,"PG 11","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",10,5.9736684963154589,{"$f":"F154*(1-Elteq!$F$6)","v":5.9736684963154589}]
["ANAMET-S",8100136,"PG 13,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",10,7.079215232025474,{"$f":"F155*(1-Elteq!$F$6)","v":7.079215232025474}]
["ANAMET-S",8100166,"PG 16","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",10,7.7574077673769963,{"$f":"F156*(1-Elteq!$F$6)","v":7.7574077673769963}]
["ANAMET-S",8100216,"PG 21","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",5,10.163597721569381,{"$f":"F157*(1-Elteq!$F$6)","v":10.163597721569381}]
["ANAMET-S",8100296,"PG 29","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",5,17.066297088229394,{"$f":"F158*(1-Elteq!$F$6)","v":17.066297088229394}]
["ANAMET-S",8100366,"PG 36","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",2,21.377000326628107,{"$f":"F159*(1-Elteq!$F$6)","v":21.377000326628107}]
["ANAMET-S",8103116,"PG 11","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",10,7.6830852977494315,{"$f":"F160*(1-Elteq!$F$6)","v":7.6830852977494315}]
["ANAMET-S",8103126,"PG 11","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",10,6.7354738099979903,{"$f":"F161*(1-Elteq!$F$6)","v":6.7354738099979903}]
["ANAMET-S",8103136,"PG 13,5","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",10,7.6830852977494315,{"$f":"F162*(1-Elteq!$F$6)","v":7.6830852977494315}]
["ANAMET-S",8103146,"PG 13,5","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",10,6.7354738099979903,{"$f":"F163*(1-Elteq!$F$6)","v":6.7354738099979903}]
["ANAMET-S",8103166,"PG 16","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",10,8.110439498107926,{"$f":"F164*(1-Elteq!$F$6)","v":8.110439498107926}]
["ANAMET-S",8103216,"PG 21","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",5,11.417789396534523,{"$f":"F165*(1-Elteq!$F$6)","v":11.417789396534523}]
["ANAMET-S",8103296,"PG 29","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",5,16.703975048795016,{"$f":"F166*(1-Elteq!$F$6)","v":16.703975048795016}]
["ANAMET-S",8103366,"PG 36","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",2,27.369249440350458,{"$f":"F167*(1-Elteq!$F$6)","v":27.369249440350458}]
["ANAMET-S",8107096,"PG 9","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",10,12.068111005775711,{"$f":"F168*(1-Elteq!$F$6)","v":12.068111005775711}]
["ANAMET-S",8107116,"PG 11","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",10,12.904238789085806,{"$f":"F169*(1-Elteq!$F$6)","v":12.904238789085806}]
["ANAMET-S",8107126,"PG 9","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",10,12.904238789085806,{"$f":"F170*(1-Elteq!$F$6)","v":12.904238789085806}]
["ANAMET-S",8107146,"PG 11","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",10,11.956627301334363,{"$f":"F171*(1-Elteq!$F$6)","v":11.956627301334363}]
["ANAMET-S",8107156,"PG 13,5","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",10,14.465010651264651,{"$f":"F172*(1-Elteq!$F$6)","v":14.465010651264651}]
["ANAMET-S",8107166,"PG 16","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",10,17.512231905994774,{"$f":"F173*(1-Elteq!$F$6)","v":17.512231905994774}]
["ANAMET-S",8107216,"PG 21","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",5,26.839701844254062,{"$f":"F174*(1-Elteq!$F$6)","v":26.839701844254062}]
["ANAMET-S",8107296,"PG 29","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",5,40.366391316470718,{"$f":"F175*(1-Elteq!$F$6)","v":40.366391316470718}]
["ANAMET-S",8120146,"M20 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",10,6.4381839314877336,{"$f":"F176*(1-Elteq!$F$6)","v":6.4381839314877336}]
["ANAMET-S",8120156,"M16 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",10,4.8959926867157808,{"$f":"F177*(1-Elteq!$F$6)","v":4.8959926867157808}]
["ANAMET-S",8120166,"M16 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",10,6.6983125751842083,{"$f":"F178*(1-Elteq!$F$6)","v":6.6983125751842083}]
["ANAMET-S",8120176,"M20 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",10,6.9863121449910182,{"$f":"F179*(1-Elteq!$F$6)","v":6.9863121449910182}]
["ANAMET-S",8120206,"M20 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",10,6.9863121449910182,{"$f":"F180*(1-Elteq!$F$6)","v":6.9863121449910182}]
["ANAMET-S",8120256,"M25 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",5,9.7734047560246697,{"$f":"F181*(1-Elteq!$F$6)","v":9.7734047560246697}]
["ANAMET-S",8120326,"M32 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",5,15.942169735112486,{"$f":"F182*(1-Elteq!$F$6)","v":15.942169735112486}]
["ANAMET-S",8120406,"M40 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with male thread, IP 40",2,21.377000326628107,{"$f":"F183*(1-Elteq!$F$6)","v":21.377000326628107}]
["ANAMET-S",8123156,"M16 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",10,6.5125064011152984,{"$f":"F184*(1-Elteq!$F$6)","v":6.5125064011152984}]
["ANAMET-S",8123166,"M16 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",10,7.4601178888667397,{"$f":"F185*(1-Elteq!$F$6)","v":7.4601178888667397}]
["ANAMET-S",8123206,"M20 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",10,7.8038593108942234,{"$f":"F186*(1-Elteq!$F$6)","v":7.8038593108942234}]
["ANAMET-S",8123256,"M25 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",5,10.981144887472585,{"$f":"F187*(1-Elteq!$F$6)","v":10.981144887472585}]
["ANAMET-S",8123326,"M32 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",5,16.062943748257275,{"$f":"F188*(1-Elteq!$F$6)","v":16.062943748257275}]
["ANAMET-S",8123406,"M40 x 1,5","Multiflex fittings for SL / SLI, Straight fixed with female thread, IP 40",2,27.369249440350458,{"$f":"F189*(1-Elteq!$F$6)","v":27.369249440350458}]
["ANAMET-S",8127156,"M16 x 1,5","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",10,10.76746778729334,{"$f":"F190*(1-Elteq!$F$6)","v":10.76746778729334}]
["ANAMET-S",8127166,"M16 x 1,5","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",10,12.904238789085806,{"$f":"F191*(1-Elteq!$F$6)","v":12.904238789085806}]
["ANAMET-S",8127176,"M20 x 1,5","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",10,12.904238789085806,{"$f":"F192*(1-Elteq!$F$6)","v":12.904238789085806}]
["ANAMET-S",8127206,"M20 x 1,5","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",10,14.465010651264651,{"$f":"F193*(1-Elteq!$F$6)","v":14.465010651264651}]
["ANAMET-S",8127256,"M25 x 1,5","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",5,23.021384967137962,{"$f":"F194*(1-Elteq!$F$6)","v":23.021384967137962}]
["ANAMET-S",8127326,"M32 x 1,5","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",5,54.905724437362927,{"$f":"F195*(1-Elteq!$F$6)","v":54.905724437362927}]
["ANAMET-S",8127406,"M40 x 1,5","Multiflex fittings for SL / SLI, Straight cablehose male thread, IP 68",2,68.460284835689919,{"$f":"F196*(1-Elteq!$F$6)","v":68.460284835689919}]
["ANAMET-S",8172106,"M32 x 1,5","Multiflex fittings for SL / SLI, Connection ring SL / SLI",10,0.74322469627564036,{"$f":"F197*(1-Elteq!$F$6)","v":0.74322469627564036}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8172356,"-","Multiflex fittings for SL / SLI, Connection ring SL / SLI",2,3.5303173073092915,{"$f":"F198*(1-Elteq!$F$6)","v":3.5303173073092915}]
["ANAMET-S",8173126,"-","Multiflex fittings for SL / SLI, Connection set for SL / SLI",10,2.8799956980681065,{"$f":"F199*(1-Elteq!$F$6)","v":2.8799956980681065}]
["ANAMET-S",8173166,"-","Multiflex fittings for SL / SLI, Connection set for SL / SLI",10,2.8799956980681065,{"$f":"F200*(1-Elteq!$F$6)","v":2.8799956980681065}]
["ANAMET-S",8173206,"-","Multiflex fittings for SL / SLI, Connection set for SL / SLI",5,3.7161234813782018,{"$f":"F201*(1-Elteq!$F$6)","v":3.7161234813782018}]
["ANAMET-S",8173266,"-","Multiflex fittings for SL / SLI, Connection set for SL / SLI",5,5.6670883091017572,{"$f":"F202*(1-Elteq!$F$6)","v":5.6670883091017572}]
["ANAMET-S",8172106,"M32 x 1,5","Multiflex fittings for SL / SLI, Connection ring SL / SLI",10,0.74322469627564036,{"$f":"F203*(1-Elteq!$F$6)","v":0.74322469627564036}]
["ANAMET-S",8172136,"-","Multiflex fittings for SL / SLI, Connection ring SL / SLI",10,0.83612778331009541,{"$f":"F204*(1-Elteq!$F$6)","v":0.83612778331009541}]
["ANAMET-S",8172166,"-","Multiflex fittings for SL / SLI, Connection ring SL / SLI",10,0.92903087034455045,{"$f":"F205*(1-Elteq!$F$6)","v":0.92903087034455045}]
["ANAMET-S",8172206,"-","Multiflex fittings for SL / SLI, Connection ring SL / SLI",5,1.161288587930688,{"$f":"F206*(1-Elteq!$F$6)","v":1.161288587930688}]
["ANAMET-S",8172266,"-","Multiflex fittings for SL / SLI, Connection ring SL / SLI",5,2.322577175861376,{"$f":"F207*(1-Elteq!$F$6)","v":2.322577175861376}]
["ANAMET-S",8172356,"-","Multiflex fittings for SL / SLI, Connection ring SL / SLI",2,3.5303173073092915,{"$f":"F208*(1-Elteq!$F$6)","v":3.5303173073092915}]
["ANAMET-S","7120169-6","M16 x 1,5","Stainless steel 304 fittings SLI, Straight fixed with male thread, IP 40",10,15.812105413264247,{"$f":"F209*(1-Elteq!$F$6)","v":15.812105413264247}]
["ANAMET-S","7120179-6","M20 x 1,5","Stainless steel 304 fittings SLI, Straight fixed with male thread, IP 40",10,21.098291065524741,{"$f":"F210*(1-Elteq!$F$6)","v":21.098291065524741}]
["ANAMET-S","7120209-6","M20 x 1,5","Stainless steel 304 fittings SLI, Straight fixed with male thread, IP 40",10,21.191194152559191,{"$f":"F211*(1-Elteq!$F$6)","v":21.191194152559191}]
["ANAMET-S","7120259-6","M25 x 1,5","Stainless steel 304 fittings SLI, Straight fixed with male thread, IP 40",5,25.278929982075219,{"$f":"F212*(1-Elteq!$F$6)","v":25.278929982075219}]
["ANAMET-S","7120329-6","M32 x 1,5","Stainless steel 304 fittings SLI, Straight fixed with male thread, IP 40",5,32.376725831507585,{"$f":"F213*(1-Elteq!$F$6)","v":32.376725831507585}]
["ANAMET-S","7120409-6","M40 x 1,5","Stainless steel 304 fittings SLI, Straight fixed with male thread, IP 40",2,47.919412292371909,{"$f":"F214*(1-Elteq!$F$6)","v":47.919412292371909}]
["ANAMET-S","7129169-6","M16 x 1,5","Stainless steel 304 fittings SLI, 90° elbow fixed with male thread, IP 40",10,31.029631069507985,{"$f":"F215*(1-Elteq!$F$6)","v":31.029631069507985}]
["ANAMET-S","7129179-6","M20 x 1,5","Stainless steel 304 fittings SLI, 90° elbow fixed with male thread, IP 40",10,31.958661939852536,{"$f":"F216*(1-Elteq!$F$6)","v":31.958661939852536}]
["ANAMET-S","7129209-6","M20 x 1,5","Stainless steel 304 fittings SLI, 90° elbow fixed with male thread, IP 40",10,35.210269986058464,{"$f":"F217*(1-Elteq!$F$6)","v":35.210269986058464}]
["ANAMET-S","7129259-6","M25 x 1,5","Stainless steel 304 fittings SLI, 90° elbow fixed with male thread, IP 40",5,45.290254929296829,{"$f":"F218*(1-Elteq!$F$6)","v":45.290254929296829}]
["ANAMET-S","7129329-6","M32 x 1,5","Stainless steel 304 fittings SLI, 90° elbow fixed with male thread, IP 40",5,68.562478231427818,{"$f":"F219*(1-Elteq!$F$6)","v":68.562478231427818}]
["ANAMET-S","7129409-6","M40 x 1,5","Stainless steel 304 fittings SLI, 90° elbow fixed with male thread, IP 40",2,88.536641943835662,{"$f":"F220*(1-Elteq!$F$6)","v":88.536641943835662}]
["ANAMET-S","7140129-6","NPT 1/2\"","Stainless steel 304 fittings SLI, Straight fixed with male thread, IP 40",10,15.812105413264247,{"$f":"F221*(1-Elteq!$F$6)","v":15.812105413264247}]
["ANAMET-S","7140169-6","NPT 1/2\"","Stainless steel 304 fittings SLI, Straight fixed with male thread, IP 40",10,21.191194152559191,{"$f":"F222*(1-Elteq!$F$6)","v":21.191194152559191}]
["ANAMET-S","7140209-6","NPT 3/4\"","Stainless steel 304 fittings SLI, Straight fixed with male thread, IP 40",5,25.278929982075219,{"$f":"F223*(1-Elteq!$F$6)","v":25.278929982075219}]
["ANAMET-S","7140269-6","NPT 1\"","Stainless steel 304 fittings SLI, Straight fixed with male thread, IP 40",5,32.376725831507585,{"$f":"F224*(1-Elteq!$F$6)","v":32.376725831507585}]
["ANAMET-S","7140359-6","NPT 1.1/4\"","Stainless steel 304 fittings SLI, Straight fixed with male thread, IP 40",2,47.919412292371909,{"$f":"F225*(1-Elteq!$F$6)","v":47.919412292371909}]
["ANAMET-S","7149129-6","NPT 1/2\"","Stainless steel 304 fittings SLI, 90° elbow fixed with male thread, IP 40",10,31.029631069507985,{"$f":"F226*(1-Elteq!$F$6)","v":31.029631069507985}]
["ANAMET-S","7149169-6","NPT 1/2\"","Stainless steel 304 fittings SLI, 90° elbow fixed with male thread, IP 40",10,35.210269986058464,{"$f":"F227*(1-Elteq!$F$6)","v":35.210269986058464}]
["ANAMET-S","7149209-6","NPT 3/4\"","Stainless steel 304 fittings SLI, 90° elbow fixed with male thread, IP 40",5,45.290254929296829,{"$f":"F228*(1-Elteq!$F$6)","v":45.290254929296829}]
["ANAMET-S","7149269-6","NPT 1\"","Stainless steel 304 fittings SLI, 90° elbow fixed with male thread, IP 40",5,68.562478231427818,{"$f":"F229*(1-Elteq!$F$6)","v":68.562478231427818}]
["ANAMET-S","7149359-6","NPT 1.1/4\"","Stainless steel 304 fittings SLI, 90° elbow fixed with male thread, IP 40",2,88.536641943835662,{"$f":"F230*(1-Elteq!$F$6)","v":88.536641943835662}]
["ANAMET-S",2605070,"PG 7","Multiflex fittings for SLI - CAP, Straight fixed with male thread, IP 40",10,4.3107032383987134,{"$f":"F231*(1-Elteq!$F$6)","v":4.3107032383987134}]
["ANAMET-S",2605090,"PG 9","Multiflex fittings for SLI - CAP, Straight fixed with male thread, IP 40",10,4.6079931169089701,{"$f":"F232*(1-Elteq!$F$6)","v":4.6079931169089701}]
["ANAMET-S",2605120,"M12 x 1,5","Multiflex fittings for SLI - CAP, Straight fixed with male thread, IP 40",10,4.6079931169089701,{"$f":"F233*(1-Elteq!$F$6)","v":4.6079931169089701}]
["ANAMET-S",2605130,"M16 x 1,5","Multiflex fittings for SLI - CAP, Straight fixed with male thread, IP 40",10,4.0134133598884576,{"$f":"F234*(1-Elteq!$F$6)","v":4.0134133598884576}]
["ANAMET-S",2615070,"PG 7","Multiflex fittings for SLI - CAP, Straight swivel with male thread, IP 40",10,4.9517345389364538,{"$f":"F235*(1-Elteq!$F$6)","v":4.9517345389364538}]
["ANAMET-S",2615090,"PG 9","Multiflex fittings for SLI - CAP, Straight swivel with male thread, IP 40",10,6.1316037442740328,{"$f":"F236*(1-Elteq!$F$6)","v":6.1316037442740328}]
["ANAMET-S",2615120,"M12 x 1,5","Multiflex fittings for SLI - CAP, Straight swivel with male thread, IP 40",10,6.5496676359290804,{"$f":"F237*(1-Elteq!$F$6)","v":6.5496676359290804}]
["ANAMET-S",2615130,"M16 x 1,5","Multiflex fittings for SLI - CAP, Straight swivel with male thread, IP 40",10,5.7135398526189851,{"$f":"F238*(1-Elteq!$F$6)","v":5.7135398526189851}]
["ANAMET-S",6000032,"3 mm","SLI-CAP conduit without cover, Stainless steel AISI-304, IP 40",30,4.1248970643298044,{"$f":"F239*(1-Elteq!$F$6)","v":4.1248970643298044}]
["ANAMET-S",6000042,"4 mm","SLI-CAP conduit without cover, Stainless steel AISI-304, IP 40",30,4.5057997211710692,{"$f":"F240*(1-Elteq!$F$6)","v":4.5057997211710692}]
["ANAMET-S",6000052,"5 mm","SLI-CAP conduit without cover, Stainless steel AISI-304, IP 40",30,4.700896203943425,{"$f":"F241*(1-Elteq!$F$6)","v":4.700896203943425}]
["ANAMET-S",6000062,"6 mm","SLI-CAP conduit without cover, Stainless steel AISI-304, IP 40",30,5.3605081218880555,{"$f":"F242*(1-Elteq!$F$6)","v":5.3605081218880555}]
["ANAMET-S",6000072,"7 mm","SLI-CAP conduit without cover, Stainless steel AISI-304, IP 40",30,5.6299270742879752,{"$f":"F243*(1-Elteq!$F$6)","v":5.6299270742879752}]
["ANAMET-S",6000082,"8 mm","SLI-CAP conduit without cover, Stainless steel AISI-304, IP 40",30,5.7507010874327671,{"$f":"F244*(1-Elteq!$F$6)","v":5.7507010874327671}]
["ANAMET-S",6000102,"10 mm","SLI-CAP conduit without cover, Stainless steel AISI-304, IP 40",30,7.00489276239791,{"$f":"F245*(1-Elteq!$F$6)","v":7.00489276239791}]
["ANAMET-S",8100072,"PG 7","Multiflex fittings for SLI - CAP, Straight fixed with male thread, IP 40",10,4.3664450906193863,{"$f":"F246*(1-Elteq!$F$6)","v":4.3664450906193863}]
["ANAMET-S",8100092,"PG 9","Multiflex fittings for SLI - CAP, Straight fixed with male thread, IP 40",10,4.3664450906193863,{"$f":"F247*(1-Elteq!$F$6)","v":4.3664450906193863}]
["ANAMET-S",8120112,"M12 x 1,5","Multiflex fittings for SLI - CAP, Straight fixed with male thread, IP 40",10,4.5057997211710692,{"$f":"F248*(1-Elteq!$F$6)","v":4.5057997211710692}]
["ANAMET-S",8120122,"M12 x 1,5","Multiflex fittings for SLI - CAP, Straight fixed with male thread, IP 40",10,4.3664450906193863,{"$f":"F249*(1-Elteq!$F$6)","v":4.3664450906193863}]
["ANAMET-S",8120132,"M16 x 1,5","Multiflex fittings for SLI - CAP, Straight fixed with male thread, IP 40",10,4.3664450906193863,{"$f":"F250*(1-Elteq!$F$6)","v":4.3664450906193863}]
["ANAMET-S",8120142,"M20 x 1,5","Multiflex fittings for SLI - CAP, Straight fixed with male thread, IP 40",10,4.5057997211710692,{"$f":"F251*(1-Elteq!$F$6)","v":4.5057997211710692}]
["ANAMET-S",8120152,"M16 x 1,5","Multiflex fittings for SLI - CAP, Straight fixed with male thread, IP 40",10,4.1527679904401404,{"$f":"F252*(1-Elteq!$F$6)","v":4.1527679904401404}]
["ANAMET-S",8172066,"-","Multiflex fittings for SLI - CAP, Connection set for SLI-CAP",10,0.74322469627564036,{"$f":"F253*(1-Elteq!$F$6)","v":0.74322469627564036}]
["ANAMET-S",8172096,"-","Multiflex fittings for SLI - CAP, Connection set for SLI-CAP",10,0.81754716590320442,{"$f":"F254*(1-Elteq!$F$6)","v":0.81754716590320442}]
["ANAMET-S",1077102,"5/16\"","SLB conduit without cover and braid, Galvanised steel, AISI-304 braid, IP 40",30,6.0851522007568049,{"$f":"F255*(1-Elteq!$F$6)","v":6.0851522007568049}]
["ANAMET-S",1077122,"3/8\"","SLB conduit without cover and braid, Galvanised steel, AISI-304 braid, IP 40",30,6.5403773272256354,{"$f":"F256*(1-Elteq!$F$6)","v":6.5403773272256354}]
["ANAMET-S",1077162,"1/2\"","SLB conduit without cover and braid, Galvanised steel, AISI-304 braid, IP 40",30,8.7514707986456646,{"$f":"F257*(1-Elteq!$F$6)","v":8.7514707986456646}]
["ANAMET-S",1077202,"3/4\"","SLB conduit without cover and braid, Galvanised steel, AISI-304 braid, IP 40",30,10.832499948217459,{"$f":"F258*(1-Elteq!$F$6)","v":10.832499948217459}]
["ANAMET-S",1077262,"1\"","SLB conduit without cover and braid, Galvanised steel, AISI-304 braid, IP 40",30,15.496234917347101,{"$f":"F259*(1-Elteq!$F$6)","v":15.496234917347101}]
["ANAMET-S",1077352,"1.1/4\"","SLB conduit without cover and braid, Galvanised steel, AISI-304 braid, IP 40",30,18.43197246763588,{"$f":"F260*(1-Elteq!$F$6)","v":18.43197246763588}]
["ANAMET-S",1077402,"1.1/2\"","SLB conduit without cover and braid, Galvanised steel, AISI-304 braid, IP 40",15,24.972349794861511,{"$f":"F261*(1-Elteq!$F$6)","v":24.972349794861511}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},1077502,"2\"","SLB conduit without cover and braid, Galvanised steel, AISI-304 braid, IP 40",15,35.024463811989548,{"$f":"F262*(1-Elteq!$F$6)","v":35.024463811989548}]
["ANAMET-S",7120140,"M20 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",10,3.9762521250746765,{"$f":"F263*(1-Elteq!$F$6)","v":3.9762521250746765}]
["ANAMET-S",7120150,"M16 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",10,3.7254137900816469,{"$f":"F264*(1-Elteq!$F$6)","v":3.7254137900816469}]
["ANAMET-S",7120161,"M16 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",10,2.7963829197370966,{"$f":"F265*(1-Elteq!$F$6)","v":2.7963829197370966}]
["ANAMET-S",7120171,"M20 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",10,3.047221254730125,{"$f":"F266*(1-Elteq!$F$6)","v":3.047221254730125}]
["ANAMET-S",7120201,"M20 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",10,3.2237371200955898,{"$f":"F267*(1-Elteq!$F$6)","v":3.2237371200955898}]
["ANAMET-S",7120251,"M25 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",5,4.9981860824536808,{"$f":"F268*(1-Elteq!$F$6)","v":4.9981860824536808}]
["ANAMET-S",7120321,"M32 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",5,7.9617945588527972,{"$f":"F269*(1-Elteq!$F$6)","v":7.9617945588527972}]
["ANAMET-S",7120401,"M40 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",2,12.839206628161687,{"$f":"F270*(1-Elteq!$F$6)","v":12.839206628161687}]
["ANAMET-S",7120501,"M50 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",2,18.023198884684277,{"$f":"F271*(1-Elteq!$F$6)","v":18.023198884684277}]
["ANAMET-S",7120631,"M63 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",2,25.827058195578502,{"$f":"F272*(1-Elteq!$F$6)","v":25.827058195578502}]
["ANAMET-S",8120161,"M16 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",10,3.8183168771161027,{"$f":"F273*(1-Elteq!$F$6)","v":3.8183168771161027}]
["ANAMET-S",8120171,"M20 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",10,4.1063164469229125,{"$f":"F274*(1-Elteq!$F$6)","v":4.1063164469229125}]
["ANAMET-S",8120201,"M20 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",10,4.1063164469229125,{"$f":"F275*(1-Elteq!$F$6)","v":4.1063164469229125}]
["ANAMET-S",8120251,"M25 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",5,6.0572812746464679,{"$f":"F276*(1-Elteq!$F$6)","v":6.0572812746464679}]
["ANAMET-S",8120321,"M32 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",5,9.7455338299143328,{"$f":"F277*(1-Elteq!$F$6)","v":9.7455338299143328}]
["ANAMET-S",8120401,"M40 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",2,17.846683019318814,{"$f":"F278*(1-Elteq!$F$6)","v":17.846683019318814}]
["ANAMET-S",8120501,"M50 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",2,23.95041583748251,{"$f":"F279*(1-Elteq!$F$6)","v":23.95041583748251}]
["ANAMET-S",8120631,"M63 x 1,5","Multiflex fittings for SLB, Straight fixed with male thread, IP 40",2,36.724590304720074,{"$f":"F280*(1-Elteq!$F$6)","v":36.724590304720074}]
["ANAMET-S",8177100,"-","Multiflex fittings for SLB, Connection set for SLB",10,1.3006432184823704,{"$f":"F281*(1-Elteq!$F$6)","v":1.3006432184823704}]
["ANAMET-S",8177120,"-","Multiflex fittings for SLB, Connection set for SLB",10,1.3006432184823704,{"$f":"F282*(1-Elteq!$F$6)","v":1.3006432184823704}]
["ANAMET-S",8177160,"-","Multiflex fittings for SLB, Connection set for SLB",10,1.4864493925512807,{"$f":"F283*(1-Elteq!$F$6)","v":1.4864493925512807}]
["ANAMET-S",8177200,"-","Multiflex fittings for SLB, Connection set for SLB",5,1.8580617406891009,{"$f":"F284*(1-Elteq!$F$6)","v":1.8580617406891009}]
["ANAMET-S",8177260,"-","Multiflex fittings for SLB, Connection set for SLB",5,2.415480262895831,{"$f":"F285*(1-Elteq!$F$6)","v":2.415480262895831}]
["ANAMET-S",8177350,"-","Multiflex fittings for SLB, Connection set for SLB",2,2.7870926110336511,{"$f":"F286*(1-Elteq!$F$6)","v":2.7870926110336511}]
["ANAMET-S",8177400,"-","Multiflex fittings for SLB, Connection set for SLB",2,3.9019296554471117,{"$f":"F287*(1-Elteq!$F$6)","v":3.9019296554471117}]
["ANAMET-S",8177500,"-","Multiflex fittings for SLB, Connection set for SLB",2,6.1316037442740328,{"$f":"F288*(1-Elteq!$F$6)","v":6.1316037442740328}]
["ANAMET-S",5120100,"5/16 \"","UI conduit without cover, Stainless steel AISI-304, IP 40",30,9.0208897510455852,{"$f":"F289*(1-Elteq!$F$6)","v":9.0208897510455852}]
["ANAMET-S",5120120,"3/8\"","UI conduit without cover, Stainless steel AISI-304, IP 40",30,9.4668245688109689,{"$f":"F290*(1-Elteq!$F$6)","v":9.4668245688109689}]
["ANAMET-S",5120160,"1/2\"","UI conduit without cover, Stainless steel AISI-304, IP 40",30,13.517399163513209,{"$f":"F291*(1-Elteq!$F$6)","v":13.517399163513209}]
["ANAMET-S",5120220,"3/4\"","UI conduit without cover, Stainless steel AISI-304, IP 40",30,19.537519203345898,{"$f":"F292*(1-Elteq!$F$6)","v":19.537519203345898}]
["ANAMET-S",5120250,"1 \"","UI conduit without cover, Stainless steel AISI-304, IP 40",30,31.763565457080176,{"$f":"F293*(1-Elteq!$F$6)","v":31.763565457080176}]
["ANAMET-S",5120340,"1 1/4\"","UI conduit without cover, Stainless steel AISI-304, IP 40",30,42.995548679545799,{"$f":"F294*(1-Elteq!$F$6)","v":42.995548679545799}]
["ANAMET-S",5120400,"1.1/2\"","UI conduit without cover, Stainless steel AISI-304, IP 40",15,59.97823298944418,{"$f":"F295*(1-Elteq!$F$6)","v":59.97823298944418}]
["ANAMET-S",5120500,"2\"","UI conduit without cover, Stainless steel AISI-304, IP 40",15,63.555001840270691,{"$f":"F296*(1-Elteq!$F$6)","v":63.555001840270691}]
["ANAMET-S",5150100,"5/16 \"","UIG conduit without cover, Galvanised steel, IP 40",30,5.5927658394741933,{"$f":"F297*(1-Elteq!$F$6)","v":5.5927658394741933}]
["ANAMET-S",5150120,"3/8\"","UIG conduit without cover, Galvanised steel, IP 40",30,5.852894483170668,{"$f":"F298*(1-Elteq!$F$6)","v":5.852894483170668}]
["ANAMET-S",5150160,"1/2\"","UIG conduit without cover, Galvanised steel, IP 40",30,6.958441218880683,{"$f":"F299*(1-Elteq!$F$6)","v":6.958441218880683}]
["ANAMET-S",5150220,"3/4\"","UIG conduit without cover, Galvanised steel, IP 40",30,7.2464407886874929,{"$f":"F300*(1-Elteq!$F$6)","v":7.2464407886874929}]
["ANAMET-S",5150250,"1 \"","UIG conduit without cover, Galvanised steel, IP 40",30,8.7607611073491096,{"$f":"F301*(1-Elteq!$F$6)","v":8.7607611073491096}]
["ANAMET-S",5150340,"1 1/4\"","UIG conduit without cover, Galvanised steel, IP 40",30,11.687208348934446,{"$f":"F302*(1-Elteq!$F$6)","v":11.687208348934446}]
["ANAMET-S",5150400,"1.1/2\"","UIG conduit without cover, Galvanised steel, IP 40",15,12.095981931886046,{"$f":"F303*(1-Elteq!$F$6)","v":12.095981931886046}]
["ANAMET-S",5150500,"2\"","UIG conduit without cover, Galvanised steel, IP 40",15,15.031719482174825,{"$f":"F304*(1-Elteq!$F$6)","v":15.031719482174825}]
["ANAMET-S",5150630,"2 1/2\"","UIG conduit without cover, Galvanised steel, IP 40",7.5,15.812105413264247,{"$f":"F305*(1-Elteq!$F$6)","v":15.812105413264247}]
["ANAMET-S",5150750,"3\"","UIG conduit without cover, Galvanised steel, IP 40",7.5,25.316091216888999,{"$f":"F306*(1-Elteq!$F$6)","v":25.316091216888999}]
["ANAMET-S",5150990,"4\"","UIG conduit without cover, Galvanised steel, IP 40",7.5,32.562532005576486,{"$f":"F307*(1-Elteq!$F$6)","v":32.562532005576486}]
["ANAMET-S",8172109,"-","Multiflex fittings for UI / UIG, Connection set for UI",10,2.1367710017924657,{"$f":"F308*(1-Elteq!$F$6)","v":2.1367710017924657}]
["ANAMET-S",8172139,"-","Multiflex fittings for UI / UIG, Connection set for UI",10,2.322577175861376,{"$f":"F309*(1-Elteq!$F$6)","v":2.322577175861376}]
["ANAMET-S",8172169,"-","Multiflex fittings for UI / UIG, Connection set for UI",10,3.0193503286197889,{"$f":"F310*(1-Elteq!$F$6)","v":3.0193503286197889}]
["ANAMET-S",8172209,"-","Multiflex fittings for UI / UIG, Connection set for UI",5,4.5522512646882971,{"$f":"F311*(1-Elteq!$F$6)","v":4.5522512646882971}]
["ANAMET-S",8172269,"-","Multiflex fittings for UI / UIG, Connection set for UI",5,7.8967623979286792,{"$f":"F312*(1-Elteq!$F$6)","v":7.8967623979286792}]
["ANAMET-S",8172359,"-","Multiflex fittings for UI / UIG, Connection set for UI",2,8.4541809201354088,{"$f":"F313*(1-Elteq!$F$6)","v":8.4541809201354088}]
["ANAMET-S",8172406,"-","Multiflex fittings for UI / UIG, Connection ring for UIG",2,5.5741852220673023,{"$f":"F314*(1-Elteq!$F$6)","v":5.5741852220673023}]
["ANAMET-S",8172409,"-","Multiflex fittings for UI / UIG, Connection set for UI",2,15.979330969926268,{"$f":"F315*(1-Elteq!$F$6)","v":15.979330969926268}]
["ANAMET-S",8172506,"-","Multiflex fittings for UI / UIG, Connection ring for UIG",2,6.6890222664807633,{"$f":"F316*(1-Elteq!$F$6)","v":6.6890222664807633}]
["ANAMET-S",8172509,"-","Multiflex fittings for UI / UIG, Connection set for UI",2,16.536749492132998,{"$f":"F317*(1-Elteq!$F$6)","v":16.536749492132998}]
["ANAMET-S",8172636,"-","Multiflex fittings for UI / UIG, Connection ring for UIG",2,17.744489623580915,{"$f":"F318*(1-Elteq!$F$6)","v":17.744489623580915}]
["ANAMET-S",8172756,"-","Multiflex fittings for UI / UIG, Connection ring for UIG",2,23.968996454889403,{"$f":"F319*(1-Elteq!$F$6)","v":23.968996454889403}]
["ANAMET-S",8172996,"-","Multiflex fittings for UI / UIG, Connection ring for UIG",2,39.483811989643392,{"$f":"F320*(1-Elteq!$F$6)","v":39.483811989643392}]
["ANAMET-S",7100117,"PG 11","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,5.1654116391156997,{"$f":"F321*(1-Elteq!$F$6)","v":5.1654116391156997}]
["ANAMET-S",7100137,"PG 13,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,5.1747019478191456,{"$f":"F322*(1-Elteq!$F$6)","v":5.1747019478191456}]
["ANAMET-S",7100167,"PG 16","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,6.3824420792670615,{"$f":"F323*(1-Elteq!$F$6)","v":6.3824420792670615}]
["ANAMET-S",7100217,"PG 21","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",5,9.6526307428798805,{"$f":"F324*(1-Elteq!$F$6)","v":9.6526307428798805}]
["ANAMET-S",7100297,"PG 29","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",5,16.202298378808958,{"$f":"F325*(1-Elteq!$F$6)","v":16.202298378808958}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},7100367,"PG 36","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",2,21.414161561441887,{"$f":"F326*(1-Elteq!$F$6)","v":21.414161561441887}]
["ANAMET-S",7100427,"PG 42","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",2,23.513771328420571,{"$f":"F327*(1-Elteq!$F$6)","v":23.513771328420571}]
["ANAMET-S",7100487,"PG 48","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40","-",32.339564596693798,{"$f":"F328*(1-Elteq!$F$6)","v":32.339564596693798}]
["ANAMET-S",7109117,"PG 11","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",10,7.3672148018322838,{"$f":"F329*(1-Elteq!$F$6)","v":7.3672148018322838}]
["ANAMET-S",7109137,"PG 13,5","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",10,7.5344403584943027,{"$f":"F330*(1-Elteq!$F$6)","v":7.5344403584943027}]
["ANAMET-S",7109167,"PG 16","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",10,8.7143095638318826,{"$f":"F331*(1-Elteq!$F$6)","v":8.7143095638318826}]
["ANAMET-S",7109217,"PG 21","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",5,12.383981501692856,{"$f":"F332*(1-Elteq!$F$6)","v":12.383981501692856}]
["ANAMET-S",7109297,"PG 29","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",5,22.045902553276179,{"$f":"F333*(1-Elteq!$F$6)","v":22.045902553276179}]
["ANAMET-S",7109367,"PG 36","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",2,35.581882334196273,{"$f":"F334*(1-Elteq!$F$6)","v":35.581882334196273}]
["ANAMET-S",7109427,"PG 42","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",2,53.289210722963411,{"$f":"F335*(1-Elteq!$F$6)","v":53.289210722963411}]
["ANAMET-S",7109487,"PG 48","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",2,74.666211049591524,{"$f":"F336*(1-Elteq!$F$6)","v":74.666211049591524}]
["ANAMET-S",7120147,"M20 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,5.3697984305915014,{"$f":"F337*(1-Elteq!$F$6)","v":5.3697984305915014}]
["ANAMET-S",7120157,"M16 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,5.1189600955984718,{"$f":"F338*(1-Elteq!$F$6)","v":5.1189600955984718}]
["ANAMET-S",7120167,"M16 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,5.1189600955984718,{"$f":"F339*(1-Elteq!$F$6)","v":5.1189600955984718}]
["ANAMET-S",7120177,"M20 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,5.3697984305915014,{"$f":"F340*(1-Elteq!$F$6)","v":5.3697984305915014}]
["ANAMET-S",7120207,"M20 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,6.2430874487153778,{"$f":"F341*(1-Elteq!$F$6)","v":6.2430874487153778}]
["ANAMET-S",7120257,"M25 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",5,9.5504373471419779,{"$f":"F342*(1-Elteq!$F$6)","v":9.5504373471419779}]
["ANAMET-S",7120327,"M32 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",5,15.858556956781475,{"$f":"F343*(1-Elteq!$F$6)","v":15.858556956781475}]
["ANAMET-S",7120407,"M40 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",2,21.293387548297098,{"$f":"F344*(1-Elteq!$F$6)","v":21.293387548297098}]
["ANAMET-S",7120507,"M50 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",2,23.597384106751576,{"$f":"F345*(1-Elteq!$F$6)","v":23.597384106751576}]
["ANAMET-S",7120637,"M63 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",2,32.516080462059264,{"$f":"F346*(1-Elteq!$F$6)","v":32.516080462059264}]
["ANAMET-S",7129147,"M20 x 1,5","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",10,8.9744382075283582,{"$f":"F347*(1-Elteq!$F$6)","v":8.9744382075283582}]
["ANAMET-S",7129157,"M16 x 1,5","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",10,8.0918588807010359,{"$f":"F348*(1-Elteq!$F$6)","v":8.0918588807010359}]
["ANAMET-S",7129167,"M16 x 1,5","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",10,7.3486341844253937,{"$f":"F349*(1-Elteq!$F$6)","v":7.3486341844253937}]
["ANAMET-S",7129177,"M20 x 1,5","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",10,8.2312135112527169,{"$f":"F350*(1-Elteq!$F$6)","v":8.2312135112527169}]
["ANAMET-S",7129207,"M20 x 1,5","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",10,9.0115994423421384,{"$f":"F351*(1-Elteq!$F$6)","v":9.0115994423421384}]
["ANAMET-S",7129257,"M25 x 1,5","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",5,14.02836614220271,{"$f":"F352*(1-Elteq!$F$6)","v":14.02836614220271}]
["ANAMET-S",7129327,"M32 x 1,5","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",5,25.148865660226978,{"$f":"F353*(1-Elteq!$F$6)","v":25.148865660226978}]
["ANAMET-S",7129407,"M40 x 1,5","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",2,36.139300856403004,{"$f":"F354*(1-Elteq!$F$6)","v":36.139300856403004}]
["ANAMET-S",7129507,"M50 x 1,5","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",2,53.289210722963411,{"$f":"F355*(1-Elteq!$F$6)","v":53.289210722963411}]
["ANAMET-S",7129637,"M63 x 1,5","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",2,72.548020665205954,{"$f":"F356*(1-Elteq!$F$6)","v":72.548020665205954}]
["ANAMET-S",8130167,"M16 x 1,5","Multiflex fittings for UI / UIG, Straight swivel with male thread, IP 40",10,8.8815351204939024,{"$f":"F357*(1-Elteq!$F$6)","v":8.8815351204939024}]
["ANAMET-S",8130207,"M20 x 1,5","Multiflex fittings for UI / UIG, Straight swivel with male thread, IP 40",10,10.470177908783082,{"$f":"F358*(1-Elteq!$F$6)","v":10.470177908783082}]
["ANAMET-S",8130257,"M25 x 1,5","Multiflex fittings for UI / UIG, Straight swivel with male thread, IP 40",5,14.36281725552675,{"$f":"F359*(1-Elteq!$F$6)","v":14.36281725552675}]
["ANAMET-S",8130327,"M32 x 1,5","Multiflex fittings for UI / UIG, Straight swivel with male thread, IP 40",5,24.21983478988243,{"$f":"F360*(1-Elteq!$F$6)","v":24.21983478988243}]
["ANAMET-S",8130407,"M40 x 1,5","Multiflex fittings for UI / UIG, Straight swivel with male thread, IP 40",2,27.304217279426339,{"$f":"F361*(1-Elteq!$F$6)","v":27.304217279426339}]
["ANAMET-S",8130507,"M50 x 1,5","Multiflex fittings for UI / UIG, Straight swivel with male thread, IP 40",2,38.787038836884982,{"$f":"F362*(1-Elteq!$F$6)","v":38.787038836884982}]
["ANAMET-S",8130637,"M63 x 1,5","Multiflex fittings for UI / UIG, Straight swivel with male thread, IP 40",2,56.187787038438401,{"$f":"F363*(1-Elteq!$F$6)","v":56.187787038438401}]
["ANAMET-S",8139157,"M16 x 1,5","Multiflex fittings for UI / UIG, 90° elbow swivel with male thread, IP 40",10,15.198945038836843,{"$f":"F364*(1-Elteq!$F$6)","v":15.198945038836843}]
["ANAMET-S",8139167,"M20 x 1,5","Multiflex fittings for UI / UIG, 90° elbow swivel with male thread, IP 40",10,13.842559968133802,{"$f":"F365*(1-Elteq!$F$6)","v":13.842559968133802}]
["ANAMET-S",8139207,"M20 x 1,5","Multiflex fittings for UI / UIG, 90° elbow swivel with male thread, IP 40",10,17.939586106353268,{"$f":"F366*(1-Elteq!$F$6)","v":17.939586106353268}]
["ANAMET-S",8139257,"M25 x 1,5","Multiflex fittings for UI / UIG, 90° elbow swivel with male thread, IP 40",5,28.511957410874249,{"$f":"F367*(1-Elteq!$F$6)","v":28.511957410874249}]
["ANAMET-S",8139327,"M32 x 1,5","Multiflex fittings for UI / UIG, 90° elbow swivel with male thread, IP 40",5,46.47012413463441,{"$f":"F368*(1-Elteq!$F$6)","v":46.47012413463441}]
["ANAMET-S",7140127,"NPT 1/2\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,5.2676050348536014,{"$f":"F369*(1-Elteq!$F$6)","v":5.2676050348536014}]
["ANAMET-S",7140167,"NPT 1/2\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,6.3917323879705075,{"$f":"F370*(1-Elteq!$F$6)","v":6.3917323879705075}]
["ANAMET-S",7140207,"NPT 3/4\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",5,9.281018394742059,{"$f":"F371*(1-Elteq!$F$6)","v":9.281018394742059}]
["ANAMET-S",7140267,"NPT 1\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",5,16.211588687512403,{"$f":"F372*(1-Elteq!$F$6)","v":16.211588687512403}]
["ANAMET-S",7140357,"NPT 1.1/4\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",2,21.980870392352063,{"$f":"F373*(1-Elteq!$F$6)","v":21.980870392352063}]
["ANAMET-S",7140407,"NPT 1.1/2\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",2,24.94447886875118,{"$f":"F374*(1-Elteq!$F$6)","v":24.94447886875118}]
["ANAMET-S",7140507,"NPT 2\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",2,37.579298705437068,{"$f":"F375*(1-Elteq!$F$6)","v":37.579298705437068}]
["ANAMET-S",7149127,"NPT 1/2\"","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",10,7.3486341844253937,{"$f":"F376*(1-Elteq!$F$6)","v":7.3486341844253937}]
["ANAMET-S",7149167,"NPT 1/2\"","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",10,9.0115994423421384,{"$f":"F377*(1-Elteq!$F$6)","v":9.0115994423421384}]
["ANAMET-S",7149207,"NPT 3/4\"","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",5,14.02836614220271,{"$f":"F378*(1-Elteq!$F$6)","v":14.02836614220271}]
["ANAMET-S",7149267,"NPT 1\"","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",5,25.148865660226978,{"$f":"F379*(1-Elteq!$F$6)","v":25.148865660226978}]
["ANAMET-S",7149357,"NPT 1.1/4\"","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",2,36.139300856403004,{"$f":"F380*(1-Elteq!$F$6)","v":36.139300856403004}]
["ANAMET-S",7149407,"NPT 1.1/2\"","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",2,53.289210722963411,{"$f":"F381*(1-Elteq!$F$6)","v":53.289210722963411}]
["ANAMET-S",7149507,"NPT 2\"","Multiflex fittings for UI / UIG, 90° elbow fixed with male thread, IP 40",2,72.548020665205954,{"$f":"F382*(1-Elteq!$F$6)","v":72.548020665205954}]
["ANAMET-S",7840107,"-","Multiflex fittings for UI / UIG, Conduit connector, IP 40",10,7.4786985062736315,{"$f":"F383*(1-Elteq!$F$6)","v":7.4786985062736315}]
["ANAMET-S",7840127,"-","Multiflex fittings for UI / UIG, Conduit connector, IP 40",10,7.4786985062736315,{"$f":"F384*(1-Elteq!$F$6)","v":7.4786985062736315}]
["ANAMET-S",7840167,"-","Multiflex fittings for UI / UIG, Conduit connector, IP 40",10,9.2903087034455041,{"$f":"F385*(1-Elteq!$F$6)","v":9.2903087034455041}]
["ANAMET-S",7840207,"-","Multiflex fittings for UI / UIG, Conduit connector, IP 40",5,13.981914598685485,{"$f":"F386*(1-Elteq!$F$6)","v":13.981914598685485}]
["ANAMET-S",7840267,"-","Multiflex fittings for UI / UIG, Conduit connector, IP 40",5,24.814414546902942,{"$f":"F387*(1-Elteq!$F$6)","v":24.814414546902942}]
["ANAMET-S",7840357,"-","Multiflex fittings for UI / UIG, Conduit connector, IP 40",2,31.150405082652778,{"$f":"F388*(1-Elteq!$F$6)","v":31.150405082652778}]
["ANAMET-S",7840407,"-","Multiflex fittings for UI / UIG, Conduit connector, IP 40",2,37.161234813782016,{"$f":"F389*(1-Elteq!$F$6)","v":37.161234813782016}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},7840507,"-","Multiflex fittings for UI / UIG, Conduit connector, IP 40",2,51.375407130053631,{"$f":"F390*(1-Elteq!$F$6)","v":51.375407130053631}]
["ANAMET-S",8120147,"M 20 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,8.20334258514238,{"$f":"F391*(1-Elteq!$F$6)","v":8.20334258514238}]
["ANAMET-S",8120157,"M16 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,6.6611513403704263,{"$f":"F392*(1-Elteq!$F$6)","v":6.6611513403704263}]
["ANAMET-S",8120167,"M16 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,6.1408940529774787,{"$f":"F393*(1-Elteq!$F$6)","v":6.1408940529774787}]
["ANAMET-S",8120177,"M20 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,6.4288936227842886,{"$f":"F394*(1-Elteq!$F$6)","v":6.4288936227842886}]
["ANAMET-S",8120207,"M20 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,7.1256667755427019,{"$f":"F395*(1-Elteq!$F$6)","v":7.1256667755427019}]
["ANAMET-S",8120257,"M25 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",5,10.609532539334765,{"$f":"F396*(1-Elteq!$F$6)","v":10.609532539334765}]
["ANAMET-S",8120327,"M 32 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",5,18.37623061541521,{"$f":"F397*(1-Elteq!$F$6)","v":18.37623061541521}]
["ANAMET-S",8120407,"M 40 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",2,26.300863939454221,{"$f":"F398*(1-Elteq!$F$6)","v":26.300863939454221}]
["ANAMET-S",8120507,"M50 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",2,39.929746807408776,{"$f":"F399*(1-Elteq!$F$6)","v":39.929746807408776}]
["ANAMET-S",8120637,"M63 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",2,53.261339796853079,{"$f":"F400*(1-Elteq!$F$6)","v":53.261339796853079}]
["ANAMET-S",8123157,"M16 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",10,8.277665054769944,{"$f":"F401*(1-Elteq!$F$6)","v":8.277665054769944}]
["ANAMET-S",8123167,"M16 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",10,6.9026993666600092,{"$f":"F402*(1-Elteq!$F$6)","v":6.9026993666600092}]
["ANAMET-S",8123207,"M20 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",10,7.9432139414459062,{"$f":"F403*(1-Elteq!$F$6)","v":7.9432139414459062}]
["ANAMET-S",8123257,"M25 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",5,11.817272670782682,{"$f":"F404*(1-Elteq!$F$6)","v":11.817272670782682}]
["ANAMET-S",8123327,"M32 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",5,18.292617837084197,{"$f":"F405*(1-Elteq!$F$6)","v":18.292617837084197}]
["ANAMET-S",8123407,"M40 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",2,32.293113053176569,{"$f":"F406*(1-Elteq!$F$6)","v":32.293113053176569}]
["ANAMET-S",8123507,"M50 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",2,47.417735622385848,{"$f":"F407*(1-Elteq!$F$6)","v":47.417735622385848}]
["ANAMET-S",8123637,"M63 x 1,5","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",2,63.861582027484388,{"$f":"F408*(1-Elteq!$F$6)","v":63.861582027484388}]
["ANAMET-S",8127157,"M16 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,12.532626440947986,{"$f":"F409*(1-Elteq!$F$6)","v":12.532626440947986}]
["ANAMET-S",8127167,"M16 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,12.346820266879075,{"$f":"F410*(1-Elteq!$F$6)","v":12.346820266879075}]
["ANAMET-S",8127177,"M20 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,12.346820266879075,{"$f":"F411*(1-Elteq!$F$6)","v":12.346820266879075}]
["ANAMET-S",8127207,"M20 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,14.604365281816333,{"$f":"F412*(1-Elteq!$F$6)","v":14.604365281816333}]
["ANAMET-S",8127257,"M25 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",5,19.305261485759761,{"$f":"F413*(1-Elteq!$F$6)","v":19.305261485759761}]
["ANAMET-S",8127327,"M32 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",5,49.23863612826117,{"$f":"F414*(1-Elteq!$F$6)","v":49.23863612826117}]
["ANAMET-S",8127407,"M40 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",2,64.929967528380629,{"$f":"F415*(1-Elteq!$F$6)","v":64.929967528380629}]
["ANAMET-S",8127507,"M50 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",2,93.367602469627315,{"$f":"F416*(1-Elteq!$F$6)","v":93.367602469627315}]
["ANAMET-S",8127637,"M63 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",2,140.5623706831305,{"$f":"F417*(1-Elteq!$F$6)","v":140.5623706831305}]
["ANAMET-S",8100097,"PG 9","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,6.8748284405496731,{"$f":"F418*(1-Elteq!$F$6)","v":6.8748284405496731}]
["ANAMET-S",8100107,"PG 9","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,6.3824420792670615,{"$f":"F419*(1-Elteq!$F$6)","v":6.3824420792670615}]
["ANAMET-S",8100117,"PG 11","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,6.4939257837084075,{"$f":"F420*(1-Elteq!$F$6)","v":6.4939257837084075}]
["ANAMET-S",8100127,"PG 11","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,7.8131496195976684,{"$f":"F421*(1-Elteq!$F$6)","v":7.8131496195976684}]
["ANAMET-S",8100137,"PG 13,5","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,6.4939257837084075,{"$f":"F422*(1-Elteq!$F$6)","v":6.4939257837084075}]
["ANAMET-S",8100167,"PG 16","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,7.8967623979286792,{"$f":"F423*(1-Elteq!$F$6)","v":7.8967623979286792}]
["ANAMET-S",8100217,"PG 21","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",5,11.027596430989814,{"$f":"F424*(1-Elteq!$F$6)","v":11.027596430989814}]
["ANAMET-S",8100297,"PG 29","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",5,19.500357968532111,{"$f":"F425*(1-Elteq!$F$6)","v":19.500357968532111}]
["ANAMET-S",8100367,"PG 36","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",2,26.300863939454221,{"$f":"F426*(1-Elteq!$F$6)","v":26.300863939454221}]
["ANAMET-S",8100427,"PG 42","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",2,39.929746807408776,{"$f":"F427*(1-Elteq!$F$6)","v":39.929746807408776}]
["ANAMET-S",8100487,"PG 48","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",2,53.261339796853079,{"$f":"F428*(1-Elteq!$F$6)","v":53.261339796853079}]
["ANAMET-S",8103117,"PG 11","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",10,7.1256667755427019,{"$f":"F429*(1-Elteq!$F$6)","v":7.1256667755427019}]
["ANAMET-S",8103127,"PG 11","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",10,8.5006324636526376,{"$f":"F430*(1-Elteq!$F$6)","v":8.5006324636526376}]
["ANAMET-S",8103137,"PG 13,5","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",10,7.8224399283011143,{"$f":"F431*(1-Elteq!$F$6)","v":7.8224399283011143}]
["ANAMET-S",8103167,"PG 16","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",10,8.2590844373630539,{"$f":"F432*(1-Elteq!$F$6)","v":8.2590844373630539}]
["ANAMET-S",8103217,"PG 21","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",5,12.281788105954957,{"$f":"F433*(1-Elteq!$F$6)","v":12.281788105954957}]
["ANAMET-S",8103297,"PG 29","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",5,19.017261915952947,{"$f":"F434*(1-Elteq!$F$6)","v":19.017261915952947}]
["ANAMET-S",8103367,"PG 36","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",2,32.293113053176569,{"$f":"F435*(1-Elteq!$F$6)","v":32.293113053176569}]
["ANAMET-S",8103427,"PG 42","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",2,50.260570085640182,{"$f":"F436*(1-Elteq!$F$6)","v":50.260570085640182}]
["ANAMET-S",8103487,"PG 48","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",2,63.861582027484388,{"$f":"F437*(1-Elteq!$F$6)","v":63.861582027484388}]
["ANAMET-S",8107097,"PG 9","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,13.833269659430355,{"$f":"F438*(1-Elteq!$F$6)","v":13.833269659430355}]
["ANAMET-S",8107117,"PG 11","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,12.346820266879075,{"$f":"F439*(1-Elteq!$F$6)","v":12.346820266879075}]
["ANAMET-S",8107127,"PG 9","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,12.346820266879075,{"$f":"F440*(1-Elteq!$F$6)","v":12.346820266879075}]
["ANAMET-S",8107157,"PG 13,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,14.604365281816333,{"$f":"F441*(1-Elteq!$F$6)","v":14.604365281816333}]
["ANAMET-S",8107167,"PG 16","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,17.651586536546457,{"$f":"F442*(1-Elteq!$F$6)","v":17.651586536546457}]
["ANAMET-S",8107217,"PG 21","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",5,27.675829627564156,{"$f":"F443*(1-Elteq!$F$6)","v":27.675829627564156}]
["ANAMET-S",8107297,"PG 29","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",5,42.596065405297637,{"$f":"F444*(1-Elteq!$F$6)","v":42.596065405297637}]
["ANAMET-S",8126157,"M16 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,19.788357538338925,{"$f":"F445*(1-Elteq!$F$6)","v":19.788357538338925}]
["ANAMET-S",8126167,"M16 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,18.41339185022899,{"$f":"F446*(1-Elteq!$F$6)","v":18.41339185022899}]
["ANAMET-S",8126177,"M20 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,18.41339185022899,{"$f":"F447*(1-Elteq!$F$6)","v":18.41339185022899}]
["ANAMET-S",8126207,"M20 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,21.692870822545252,{"$f":"F448*(1-Elteq!$F$6)","v":21.692870822545252}]
["ANAMET-S",8126227,"M25 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,26.783959992033385,{"$f":"F449*(1-Elteq!$F$6)","v":26.783959992033385}]
["ANAMET-S",8126287,"M32 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",5,38.220330005974802,{"$f":"F450*(1-Elteq!$F$6)","v":38.220330005974802}]
["ANAMET-S",8126357,"M40 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",5,60.182619780919978,{"$f":"F451*(1-Elteq!$F$6)","v":60.182619780919978}]
["ANAMET-S",8140117,"NPT 1/2\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,7.9246333240390143,{"$f":"F452*(1-Elteq!$F$6)","v":7.9246333240390143}]
["ANAMET-S",8140127,"NPT 1/2\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,6.8097962796255542,{"$f":"F453*(1-Elteq!$F$6)","v":6.8097962796255542}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8140167,"NPT 1/2\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",10,7.7666980760804405,{"$f":"F454*(1-Elteq!$F$6)","v":7.7666980760804405}]
["ANAMET-S",8140207,"NPT 3/4\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",5,10.665274391555439,{"$f":"F455*(1-Elteq!$F$6)","v":10.665274391555439}]
["ANAMET-S",8140267,"NPT 1 \"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",5,18.078940736904951,{"$f":"F456*(1-Elteq!$F$6)","v":18.078940736904951}]
["ANAMET-S",8140357,"NPT 1.1/4 \"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",2,26.951185548695406,{"$f":"F457*(1-Elteq!$F$6)","v":26.951185548695406}]
["ANAMET-S",8140407,"NPT 1.1/2\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",2,42.373097996414941,{"$f":"F458*(1-Elteq!$F$6)","v":42.373097996414941}]
["ANAMET-S",8140507,"NPT 2\"","Multiflex fittings for UI / UIG, Straight fixed with male thread, IP 40",2,58.02726816172062,{"$f":"F459*(1-Elteq!$F$6)","v":58.02726816172062}]
["ANAMET-S","8107117-3","PG 11","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,29.79402001194973,{"$f":"F460*(1-Elteq!$F$6)","v":29.79402001194973}]
["ANAMET-S","8107157-3","PG 13,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,30.490793164708144,{"$f":"F461*(1-Elteq!$F$6)","v":30.490793164708144}]
["ANAMET-S","8107167-3","PG 16","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,39.948327424815673,{"$f":"F462*(1-Elteq!$F$6)","v":39.948327424815673}]
["ANAMET-S","8107217-3","PG 21","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",5,41.314002804222156,{"$f":"F463*(1-Elteq!$F$6)","v":41.314002804222156}]
["ANAMET-S","8127157-3","M16 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,31.168985700059665,{"$f":"F464*(1-Elteq!$F$6)","v":31.168985700059665}]
["ANAMET-S","8127167-3","M16 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,29.79402001194973,{"$f":"F465*(1-Elteq!$F$6)","v":29.79402001194973}]
["ANAMET-S","8127207-3","M20 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,30.490793164708144,{"$f":"F466*(1-Elteq!$F$6)","v":30.490793164708144}]
["ANAMET-S","8127227-3","M25 x 1,5","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,39.781101868153648,{"$f":"F467*(1-Elteq!$F$6)","v":39.781101868153648}]
["ANAMET-S",2930407,"M 50 x 1,5","Multiflex fittings for  UIG, Straight fixed with male thread, IP 40",1,18.348359689304871,{"$f":"F468*(1-Elteq!$F$6)","v":18.348359689304871}]
["ANAMET-S",2930507,"M 63 x 1,5","Multiflex fittings for  UIG, Straight fixed with male thread, IP 40",1,24.470673124875461,{"$f":"F469*(1-Elteq!$F$6)","v":24.470673124875461}]
["ANAMET-S",2940637,"NPT 2 1/2\"","Multiflex fittings for  UIG, Straight fixed with male thread, IP 40",1,55.825464999004033,{"$f":"F470*(1-Elteq!$F$6)","v":55.825464999004033}]
["ANAMET-S",2940757,"NPT 3\"","Multiflex fittings for  UIG, Straight fixed with male thread, IP 40",1,73.477051535550501,{"$f":"F471*(1-Elteq!$F$6)","v":73.477051535550501}]
["ANAMET-S",2940997,"NPT 4\"","Multiflex fittings for  UIG, Straight fixed with male thread, IP 40",1,106.07674477594078,{"$f":"F472*(1-Elteq!$F$6)","v":106.07674477594078}]
["ANAMET-S",7120168,"M16 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",10,17.391457892849985,{"$f":"F473*(1-Elteq!$F$6)","v":17.391457892849985}]
["ANAMET-S",7120178,"M20 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",10,22.58474045807602,{"$f":"F474*(1-Elteq!$F$6)","v":22.58474045807602}]
["ANAMET-S",7120208,"M20 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",10,23.28151361083443,{"$f":"F475*(1-Elteq!$F$6)","v":23.28151361083443}]
["ANAMET-S",7120258,"M25 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",5,28.669892658832826,{"$f":"F476*(1-Elteq!$F$6)","v":28.669892658832826}]
["ANAMET-S",7120328,"M32 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",5,37.950911053574885,{"$f":"F477*(1-Elteq!$F$6)","v":37.950911053574885}]
["ANAMET-S",7120408,"M40 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",2,52.843275905198027,{"$f":"F478*(1-Elteq!$F$6)","v":52.843275905198027}]
["ANAMET-S",7120508,"M50 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",2,72.064924612626768,{"$f":"F479*(1-Elteq!$F$6)","v":72.064924612626768}]
["ANAMET-S",7120638,"M63 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",2,101.53378381995593,{"$f":"F480*(1-Elteq!$F$6)","v":101.53378381995593}]
["ANAMET-S",7129168,"M16 x 1,5","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",10,32.516080462059264,{"$f":"F481*(1-Elteq!$F$6)","v":32.516080462059264}]
["ANAMET-S",7129178,"M20 x 1,5","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",10,33.445111332403819,{"$f":"F482*(1-Elteq!$F$6)","v":33.445111332403819}]
["ANAMET-S",7129208,"M20 x 1,5","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",10,37.300589444333696,{"$f":"F483*(1-Elteq!$F$6)","v":37.300589444333696}]
["ANAMET-S",7129258,"M25 x 1,5","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",5,48.681217606054439,{"$f":"F484*(1-Elteq!$F$6)","v":48.681217606054439}]
["ANAMET-S",7129328,"M32 x 1,5","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",5,74.136663453495117,{"$f":"F485*(1-Elteq!$F$6)","v":74.136663453495117}]
["ANAMET-S",7129408,"M40 x 1,5","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",2,93.460505556661772,{"$f":"F486*(1-Elteq!$F$6)","v":93.460505556661772}]
["ANAMET-S",7129508,"M50 x 1,5","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",2,137.68237498506238,{"$f":"F487*(1-Elteq!$F$6)","v":137.68237498506238}]
["ANAMET-S",7129638,"M63 x 1,5","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",2,191.19455311690848,{"$f":"F488*(1-Elteq!$F$6)","v":191.19455311690848}]
["ANAMET-S",7140128,"NPT 1/2\"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",10,17.391457892849985,{"$f":"F489*(1-Elteq!$F$6)","v":17.391457892849985}]
["ANAMET-S",7140168,"NPT 1/2\"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",10,23.28151361083443,{"$f":"F490*(1-Elteq!$F$6)","v":23.28151361083443}]
["ANAMET-S",7140208,"NPT 3/4\"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",5,28.669892658832826,{"$f":"F491*(1-Elteq!$F$6)","v":28.669892658832826}]
["ANAMET-S",7140268,"NPT 1\"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",5,37.950911053574885,{"$f":"F492*(1-Elteq!$F$6)","v":37.950911053574885}]
["ANAMET-S",7140358,"NPT 1.1/4\"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",2,52.843275905198027,{"$f":"F493*(1-Elteq!$F$6)","v":52.843275905198027}]
["ANAMET-S",7140408,"NPT 1.1/2\"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",2,72.064924612626768,{"$f":"F494*(1-Elteq!$F$6)","v":72.064924612626768}]
["ANAMET-S",7140508,"NPT 2\"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",2,101.53378381995593,{"$f":"F495*(1-Elteq!$F$6)","v":101.53378381995593}]
["ANAMET-S",8143117,"NPT 1/2\"","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",10,8.5006324636526376,{"$f":"F496*(1-Elteq!$F$6)","v":8.5006324636526376}]
["ANAMET-S",8143127,"NPT 1/2\"","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",10,7.1256667755427019,{"$f":"F497*(1-Elteq!$F$6)","v":7.1256667755427019}]
["ANAMET-S",8143167,"NPT 1/2\"","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",10,8.1754716590320449,{"$f":"F498*(1-Elteq!$F$6)","v":8.1754716590320449}]
["ANAMET-S",8143207,"NPT 3/4\"","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",5,12.17030440151361,{"$f":"F499*(1-Elteq!$F$6)","v":12.17030440151361}]
["ANAMET-S",8143267,"NPT 1 \"","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",5,18.785004198366806,{"$f":"F500*(1-Elteq!$F$6)","v":18.785004198366806}]
["ANAMET-S",8143357,"NPT 1.1/4 \"","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",2,32.488209535948926,{"$f":"F501*(1-Elteq!$F$6)","v":32.488209535948926}]
["ANAMET-S",8143407,"NPT 1.1/2\"","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",2,51.11527848635717,{"$f":"F502*(1-Elteq!$F$6)","v":51.11527848635717}]
["ANAMET-S",8143507,"NPT 2\"","Multiflex fittings for UI / UIG, Straight fixed with female thread, IP 40",2,69.965314845648095,{"$f":"F503*(1-Elteq!$F$6)","v":69.965314845648095}]
["ANAMET-S",8147097,"NPT 3/8\"","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,13.721785954989009,{"$f":"F504*(1-Elteq!$F$6)","v":13.721785954989009}]
["ANAMET-S",8147107,"NPT 3/8\"","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,12.346820266879075,{"$f":"F505*(1-Elteq!$F$6)","v":12.346820266879075}]
["ANAMET-S",8147127,"NPT 1/2\"","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,12.346820266879075,{"$f":"F506*(1-Elteq!$F$6)","v":12.346820266879075}]
["ANAMET-S",8147157,"NPT 1/2\"","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",10,17.651586536546457,{"$f":"F507*(1-Elteq!$F$6)","v":17.651586536546457}]
["ANAMET-S",8147217,"NPT 3/4\"","Multiflex fittings for UI / UIG, Straight cablehose male thread, IP 68",5,27.675829627564156,{"$f":"F508*(1-Elteq!$F$6)","v":27.675829627564156}]
["ANAMET-S",7149128,"NPT 1/2\"","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",10,32.516080462059264,{"$f":"F509*(1-Elteq!$F$6)","v":32.516080462059264}]
["ANAMET-S",7149168,"NPT 1/2\"","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",10,37.300589444333696,{"$f":"F510*(1-Elteq!$F$6)","v":37.300589444333696}]
["ANAMET-S",7149208,"NPT 3/4\"","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",5,48.681217606054439,{"$f":"F511*(1-Elteq!$F$6)","v":48.681217606054439}]
["ANAMET-S",7149268,"NPT 1 \"","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",5,74.136663453495117,{"$f":"F512*(1-Elteq!$F$6)","v":74.136663453495117}]
["ANAMET-S",7149358,"NPT 1.1/4 \"","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",2,93.460505556661772,{"$f":"F513*(1-Elteq!$F$6)","v":93.460505556661772}]
["ANAMET-S",7149408,"NPT 1.1/2\"","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",2,137.68237498506238,{"$f":"F514*(1-Elteq!$F$6)","v":137.68237498506238}]
["ANAMET-S",7149508,"NPT 2\"","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",2,191.19455311690848,{"$f":"F515*(1-Elteq!$F$6)","v":191.19455311690848}]
["ANAMET-S",8100118,"PG 11","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",10,20.048486182035397,{"$f":"F516*(1-Elteq!$F$6)","v":20.048486182035397}]
["ANAMET-S",8100128,"PG 11","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",10,21.423451870145332,{"$f":"F517*(1-Elteq!$F$6)","v":21.423451870145332}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8100168,"PG 16","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",10,28.00099043218475,{"$f":"F518*(1-Elteq!$F$6)","v":28.00099043218475}]
["ANAMET-S",8100218,"PG 21","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",5,33.277885775741794,{"$f":"F519*(1-Elteq!$F$6)","v":33.277885775741794}]
["ANAMET-S",8109118,"PG 11","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",10,32.962015279824641,{"$f":"F520*(1-Elteq!$F$6)","v":32.962015279824641}]
["ANAMET-S",8109128,"PG 11","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",10,34.336980967934586,{"$f":"F521*(1-Elteq!$F$6)","v":34.336980967934586}]
["ANAMET-S",8109168,"PG 16","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",10,46.200705182234486,{"$f":"F522*(1-Elteq!$F$6)","v":46.200705182234486}]
["ANAMET-S",8109218,"PG 21","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",5,54.199660975901075,{"$f":"F523*(1-Elteq!$F$6)","v":54.199660975901075}]
["ANAMET-S",8120148,"M20 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",10,21.423451870145332,{"$f":"F524*(1-Elteq!$F$6)","v":21.423451870145332}]
["ANAMET-S",8120158,"M16 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",10,21.423451870145332,{"$f":"F525*(1-Elteq!$F$6)","v":21.423451870145332}]
["ANAMET-S",8120168,"M16 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",10,20.048486182035397,{"$f":"F526*(1-Elteq!$F$6)","v":20.048486182035397}]
["ANAMET-S",8120178,"M20 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",10,27.304217279426339,{"$f":"F527*(1-Elteq!$F$6)","v":27.304217279426339}]
["ANAMET-S",8120208,"M20 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",10,28.00099043218475,{"$f":"F528*(1-Elteq!$F$6)","v":28.00099043218475}]
["ANAMET-S",8120258,"M25 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",5,33.277885775741794,{"$f":"F529*(1-Elteq!$F$6)","v":33.277885775741794}]
["ANAMET-S",8120328,"M 32 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",5,44.119676032662703,{"$f":"F530*(1-Elteq!$F$6)","v":44.119676032662703}]
["ANAMET-S",8120408,"M40 x 1,5","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",2,82.274973877713393,{"$f":"F531*(1-Elteq!$F$6)","v":82.274973877713393}]
["ANAMET-S",8127158,"M16 x 1,5","Stainless steel 316 fittings for UI, Straight cablehose male thread, IP 68",10,40.570778107946516,{"$f":"F532*(1-Elteq!$F$6)","v":40.570778107946516}]
["ANAMET-S",8127168,"M16 x 1,5","Stainless steel 316 fittings for UI, Straight cablehose male thread, IP 68",10,39.195812419836578,{"$f":"F533*(1-Elteq!$F$6)","v":39.195812419836578}]
["ANAMET-S",8127178,"M20 x 1,5","Stainless steel 316 fittings for UI, Straight cablehose male thread, IP 68",10,41.81567947420821,{"$f":"F534*(1-Elteq!$F$6)","v":41.81567947420821}]
["ANAMET-S",8127208,"M20 x 1,5","Stainless steel 316 fittings for UI, Straight cablehose male thread, IP 68",10,46.767414013144666,{"$f":"F535*(1-Elteq!$F$6)","v":46.767414013144666}]
["ANAMET-S",8140118,"NPT 1/2\"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",10,22.259579653455429,{"$f":"F536*(1-Elteq!$F$6)","v":22.259579653455429}]
["ANAMET-S",8140128,"NPT 1/2\"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",10,20.884613965345494,{"$f":"F537*(1-Elteq!$F$6)","v":20.884613965345494}]
["ANAMET-S",8140168,"NPT 1/2\"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",10,29.190149946225773,{"$f":"F538*(1-Elteq!$F$6)","v":29.190149946225773}]
["ANAMET-S",8140208,"NPT 3/4\"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",5,34.643561155148284,{"$f":"F539*(1-Elteq!$F$6)","v":34.643561155148284}]
["ANAMET-S",8140268,"NPT 1 \"","Stainless steel 304 fittings for UI, Straight fixed with male thread, IP 40",5,41.63916360884275,{"$f":"F540*(1-Elteq!$F$6)","v":41.63916360884275}]
["ANAMET-S",8149118,"NPT 1/2\"","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",10,35.730527273451408,{"$f":"F541*(1-Elteq!$F$6)","v":35.730527273451408}]
["ANAMET-S",8149128,"NPT 1/2\"","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",10,34.355561585341476,{"$f":"F542*(1-Elteq!$F$6)","v":34.355561585341476}]
["ANAMET-S",8149168,"NPT 1/2\"","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",10,48.179540936068385,{"$f":"F543*(1-Elteq!$F$6)","v":48.179540936068385}]
["ANAMET-S",8149208,"NPT 3/4\"","Stainless steel 304 fittings for UI, 90° elbow fixed with male thread, IP 40",5,56.457205990838325,{"$f":"F544*(1-Elteq!$F$6)","v":56.457205990838325}]
["ANAMET-S",5110100,"5/16 \"","UI-CAP conduit without cover, Stainless steel AISI-304, IP 40",1,9.0208897510455852,{"$f":"F545*(1-Elteq!$F$6)","v":9.0208897510455852}]
["ANAMET-S",5750300,"ID 5,2 mm","UI-CAP conduit without cover, Stainless steel AISI-304, IP 40",1,7.2557310973909388,{"$f":"F546*(1-Elteq!$F$6)","v":7.2557310973909388}]
["ANAMET-S",5750400,"ID 5,5 mm","UI-CAP conduit without cover, Stainless steel AISI-304, IP 40",1,7.6180531368253126,{"$f":"F547*(1-Elteq!$F$6)","v":7.6180531368253126}]
["ANAMET-S",5750450,"ID 7 mm","UI-CAP conduit without cover, Stainless steel AISI-304, IP 40",1,9.1137928380800393,{"$f":"F548*(1-Elteq!$F$6)","v":9.1137928380800393}]
["ANAMET-S",5750600,"ID 6 mm","UI-CAP conduit without cover, Stainless steel AISI-304, IP 40",1,8.0546976458872521,{"$f":"F549*(1-Elteq!$F$6)","v":8.0546976458872521}]
["ANAMET-S",5751450,"ID 4,5 mm","UI-CAP conduit without cover, Stainless steel AISI-304, IP 40",1,7.2557310973909388,{"$f":"F550*(1-Elteq!$F$6)","v":7.2557310973909388}]
["ANAMET-S",5758400,"ID 8 mm","UI-CAP conduit without cover, Stainless steel AISI-304, IP 40",1,7.2743117147978298,{"$f":"F551*(1-Elteq!$F$6)","v":7.2743117147978298}]
["ANAMET-S",7121168,"M16 x 1,5","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",10,21.915838231427944,{"$f":"F552*(1-Elteq!$F$6)","v":21.915838231427944}]
["ANAMET-S",7121178,"M20 x 1,5","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",10,28.660602350129381,{"$f":"F553*(1-Elteq!$F$6)","v":28.660602350129381}]
["ANAMET-S",7121208,"M20 x 1,5","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",10,29.357375502887791,{"$f":"F554*(1-Elteq!$F$6)","v":29.357375502887791}]
["ANAMET-S",7121258,"M25 x 1,5","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",5,35.907043138816874,{"$f":"F555*(1-Elteq!$F$6)","v":35.907043138816874}]
["ANAMET-S",7121328,"M32 x 1,5","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",5,46.971800804620472,{"$f":"F556*(1-Elteq!$F$6)","v":46.971800804620472}]
["ANAMET-S",7121408,"M40 x 1,5","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",2,66.156288277235433,{"$f":"F557*(1-Elteq!$F$6)","v":66.156288277235433}]
["ANAMET-S",7121508,"M50 x 1,5","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",2,102.41636314678325,{"$f":"F558*(1-Elteq!$F$6)","v":102.41636314678325}]
["ANAMET-S",7121638,"M63 x 1,5","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",2,139.83772660426175,{"$f":"F559*(1-Elteq!$F$6)","v":139.83772660426175}]
["ANAMET-S",7141128,"NPT 1/2\"","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",10,21.915838231427944,{"$f":"F560*(1-Elteq!$F$6)","v":21.915838231427944}]
["ANAMET-S",7141168,"NPT 1/2\"","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",10,29.357375502887791,{"$f":"F561*(1-Elteq!$F$6)","v":29.357375502887791}]
["ANAMET-S",7141208,"NPT 3/4\"","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",5,35.907043138816874,{"$f":"F562*(1-Elteq!$F$6)","v":35.907043138816874}]
["ANAMET-S",7141268,"NPT 1 \"","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",5,46.971800804620472,{"$f":"F563*(1-Elteq!$F$6)","v":46.971800804620472}]
["ANAMET-S",7141358,"NPT 1.1/4 \"","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",2,66.156288277235433,{"$f":"F564*(1-Elteq!$F$6)","v":66.156288277235433}]
["ANAMET-S",7141408,"NPT 1.1/2\"","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",2,102.41636314678325,{"$f":"F565*(1-Elteq!$F$6)","v":102.41636314678325}]
["ANAMET-S",7141508,"NPT 2\"","Stainless steel 316 fittings for UI, Straight fixed with male thread, IP 40",2,139.83772660426175,{"$f":"F566*(1-Elteq!$F$6)","v":139.83772660426175}]
["ANAMET-S",8100072,"PG 7","Multiflex fittings for UI - CAP, Straight fixed with male thread, IP 40",10,4.3664450906193863,{"$f":"F567*(1-Elteq!$F$6)","v":4.3664450906193863}]
["ANAMET-S",8100092,"PG 9","Multiflex fittings for UI - CAP, Straight fixed with male thread, IP 40",10,4.3664450906193863,{"$f":"F568*(1-Elteq!$F$6)","v":4.3664450906193863}]
["ANAMET-S",8120112,"M12 x 1,5","Multiflex fittings for UI - CAP, Straight fixed with male thread, IP 40",10,4.5057997211710692,{"$f":"F569*(1-Elteq!$F$6)","v":4.5057997211710692}]
["ANAMET-S",8120122,"M12 x 1,5","Multiflex fittings for UI - CAP, Straight fixed with male thread, IP 40",10,4.3664450906193863,{"$f":"F570*(1-Elteq!$F$6)","v":4.3664450906193863}]
["ANAMET-S",8120132,"M16 x 1,5","Multiflex fittings for UI - CAP, Straight fixed with male thread, IP 40",10,4.3664450906193863,{"$f":"F571*(1-Elteq!$F$6)","v":4.3664450906193863}]
["ANAMET-S",8120142,"M20 x 1,5","Multiflex fittings for UI - CAP, Straight fixed with male thread, IP 40",10,4.5057997211710692,{"$f":"F572*(1-Elteq!$F$6)","v":4.5057997211710692}]
["ANAMET-S",8120152,"M16 x 1,5","Multiflex fittings for UI - CAP, Straight fixed with male thread, IP 40",10,4.1527679904401404,{"$f":"F573*(1-Elteq!$F$6)","v":4.1527679904401404}]
["ANAMET-S",8172069,"-","Multiflex fittings for  UI-CAP, Connection ring for UI-CAP",10,0.74322469627564036,{"$f":"F574*(1-Elteq!$F$6)","v":0.74322469627564036}]
["ANAMET-S",8172099,"-","Multiflex fittings for  UI-CAP, Connection ring for UI-CAP",10,2.5083833499302863,{"$f":"F575*(1-Elteq!$F$6)","v":2.5083833499302863}]
["ANAMET-S",432310,"PG 7","Multiflex fittings for  UI-CAP, Straight fixed with male thread, IP 40",10,5.0910891694881366,{"$f":"F576*(1-Elteq!$F$6)","v":5.0910891694881366}]
["ANAMET-S",555810,"M 12 x 1,5","Multiflex fittings for  UI-CAP, Straight fixed with male thread, IP 40",10,5.6670883091017572,{"$f":"F577*(1-Elteq!$F$6)","v":5.6670883091017572}]
["ANAMET-S",559730,"M 12 x 1,5","Multiflex fittings for  UI-CAP, Straight swivel with male thread, IP 40",10,14.975977629954155,{"$f":"F578*(1-Elteq!$F$6)","v":14.975977629954155}]
["ANAMET-S",559830,"M 16 x 1,5","Multiflex fittings for  UI-CAP, Straight swivel with male thread, IP 40",10,14.975977629954155,{"$f":"F579*(1-Elteq!$F$6)","v":14.975977629954155}]
["ANAMET-S",572610,"M 12 x 1,5","Multiflex fittings for  UI-CAP, Straight fixed with male thread, IP 40",10,5.1561213304122546,{"$f":"F580*(1-Elteq!$F$6)","v":5.1561213304122546}]
["ANAMET-S",594010,"-","Multiflex fittings for  UI-CAP, Connection ring for UI-CAP",10,1.7001264927305273,{"$f":"F581*(1-Elteq!$F$6)","v":1.7001264927305273}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},2227031,"-","Multiflex fittings for  UI-CAP, Connection ring for UI-CAP",10,0.99406303126866913,{"$f":"F582*(1-Elteq!$F$6)","v":0.99406303126866913}]
["ANAMET-S",2960120,"NPT 1/2\"","Multiflex fittings for  RWA, Straight fixed with male thread, IP 40",25,1.3006432184823704,{"$f":"F583*(1-Elteq!$F$6)","v":1.3006432184823704}]
["ANAMET-S",2960160,"NPT 1/2\"","Multiflex fittings for  RWA, Straight fixed with male thread, IP 40",25,1.5793524795857357,{"$f":"F584*(1-Elteq!$F$6)","v":1.5793524795857357}]
["ANAMET-S",2960200,"NPT 3/4\"","Multiflex fittings for  RWA, Straight fixed with male thread, IP 40",25,1.7837392710615367,{"$f":"F585*(1-Elteq!$F$6)","v":1.7837392710615367}]
["ANAMET-S",2960260,"NPT 1\"","Multiflex fittings for  RWA, Straight fixed with male thread, IP 40",10,5.78786232224655,{"$f":"F586*(1-Elteq!$F$6)","v":5.78786232224655}]
["ANAMET-S",2960350,"NPT 1 1/4\"","Multiflex fittings for  RWA, Straight fixed with male thread, IP 40",10,12.755593849830678,{"$f":"F587*(1-Elteq!$F$6)","v":12.755593849830678}]
["ANAMET-S",2960400,"NPT 1 1/2\"","Multiflex fittings for  RWA, Straight fixed with male thread, IP 40",5,17.846683019318814,{"$f":"F588*(1-Elteq!$F$6)","v":17.846683019318814}]
["ANAMET-S",2960500,"NPT 2\"","Multiflex fittings for  RWA, Straight fixed with male thread, IP 40",5,26.579573200557586,{"$f":"F589*(1-Elteq!$F$6)","v":26.579573200557586}]
["ANAMET-S",2961125,"NPT 1/2\"","Multiflex fittings for  RWA, Straight fixed with male thread, IP 40",50,0.88257932682732287,{"$f":"F590*(1-Elteq!$F$6)","v":0.88257932682732287}]
["ANAMET-S",2961165,"NPT 1/2\"","Multiflex fittings for  RWA, Straight fixed with male thread, IP 40",50,0.88257932682732287,{"$f":"F591*(1-Elteq!$F$6)","v":0.88257932682732287}]
["ANAMET-S",2961205,"NPT 3/4\"","Multiflex fittings for  RWA, Straight fixed with male thread, IP 40",25,1.4957397012547262,{"$f":"F592*(1-Elteq!$F$6)","v":1.4957397012547262}]
["ANAMET-S",2962160,"-","Multiflex fittings for  RWA, Conduit isolation bushing for RWA",1000,0.29728987851025612,{"$f":"F593*(1-Elteq!$F$6)","v":0.29728987851025612}]
["ANAMET-S",2962200,"-","Multiflex fittings for  RWA, Conduit isolation bushing for RWA",600,0.3344511133240381,{"$f":"F594*(1-Elteq!$F$6)","v":0.3344511133240381}]
["ANAMET-S",2964120,"-","Multiflex fittings for  RWA, Conduit isolation bushing for RWA",1000,0.29728987851025612,{"$f":"F595*(1-Elteq!$F$6)","v":0.29728987851025612}]
["ANAMET-S",2969120,"NPT 1/2\"","Multiflex fittings for  RWA, 90° elbow fixed with male thread, IP 40",25,1.6072234056960721,{"$f":"F596*(1-Elteq!$F$6)","v":1.6072234056960721}]
["ANAMET-S",2969160,"NPT 1/2\"","Multiflex fittings for  RWA, 90° elbow fixed with male thread, IP 40",25,2.6477379804819687,{"$f":"F597*(1-Elteq!$F$6)","v":2.6477379804819687}]
["ANAMET-S",2969200,"NPT 3/4\"","Multiflex fittings for  RWA, 90° elbow fixed with male thread, IP 40",25,4.2921226209918233,{"$f":"F598*(1-Elteq!$F$6)","v":4.2921226209918233}]
["ANAMET-S",2969260,"NPT 1\"","Multiflex fittings for  RWA, 90° elbow fixed with male thread, IP 40",10,13.294431754630518,{"$f":"F599*(1-Elteq!$F$6)","v":13.294431754630518}]
["ANAMET-S",2969350,"NPT 1 1/4\"","Multiflex fittings for  RWA, 90° elbow fixed with male thread, IP 40",10,21.646419279028024,{"$f":"F600*(1-Elteq!$F$6)","v":21.646419279028024}]
["ANAMET-S",2969400,"NPT 1 1/2\"","Multiflex fittings for  RWA, 90° elbow fixed with male thread, IP 40",5,55.621078207528228,{"$f":"F601*(1-Elteq!$F$6)","v":55.621078207528228}]
["ANAMET-S",2969500,"NPT 2\"","Multiflex fittings for  RWA, 90° elbow fixed with male thread, IP 40",5,56.568689695279673,{"$f":"F602*(1-Elteq!$F$6)","v":56.568689695279673}]
["ANAMET-S",3320121,"3/8\"","RWA conduit without cover, Aluminium steel, IP 40",30,2.9636084763991155,{"$f":"F603*(1-Elteq!$F$6)","v":2.9636084763991155}]
["ANAMET-S",3320161,"1/2\"","RWA conduit without cover, Aluminium steel, IP 40",30,3.3259305158334906,{"$f":"F604*(1-Elteq!$F$6)","v":3.3259305158334906}]
["ANAMET-S",3320201,"3/4\"","RWA conduit without cover, Aluminium steel, IP 40",30,4.4779287950607332,{"$f":"F605*(1-Elteq!$F$6)","v":4.4779287950607332}]
["ANAMET-S",3320261,"1\"","RWA conduit without cover, Aluminium steel, IP 40",15,8.7886320334594465,{"$f":"F606*(1-Elteq!$F$6)","v":8.7886320334594465}]
["ANAMET-S",3320351,"1.1/4\"","RWA conduit without cover, Aluminium steel, IP 40",15,11.492111866162089,{"$f":"F607*(1-Elteq!$F$6)","v":11.492111866162089}]
["ANAMET-S",3320401,"1.1/2\"","RWA conduit without cover, Aluminium steel, IP 40",7.5,19.937002477594053,{"$f":"F608*(1-Elteq!$F$6)","v":19.937002477594053}]
["ANAMET-S",3320501,"2\"","RWA conduit without cover, Aluminium steel, IP 40",7.5,24.210544481178982,{"$f":"F609*(1-Elteq!$F$6)","v":24.210544481178982}]
["ANAMET-S",8834160,"-","Multiflex fittings for  RWA, Conduit connector, IP 40",25,2.1460613104959116,{"$f":"F610*(1-Elteq!$F$6)","v":2.1460613104959116}]
["ANAMET-S",8834200,"-","Multiflex fittings for  RWA, Conduit connector, IP 40",10,3.455994837681728,{"$f":"F611*(1-Elteq!$F$6)","v":3.455994837681728}]
["ANAMET-S",8834260,"-","Multiflex fittings for  RWA, Conduit connector, IP 40",10,6.958441218880683,{"$f":"F612*(1-Elteq!$F$6)","v":6.958441218880683}]
["ANAMET-S",8834350,"-","Multiflex fittings for  RWA, Conduit connector, IP 40",5,13.731076263692454,{"$f":"F613*(1-Elteq!$F$6)","v":13.731076263692454}]
["ANAMET-S",8834400,"-","Multiflex fittings for  RWA, Conduit connector, IP 40",5,18.599198024297898,{"$f":"F614*(1-Elteq!$F$6)","v":18.599198024297898}]
["ANAMET-S",8834500,"-","Multiflex fittings for  RWA, Conduit connector, IP 40",2,36.603816291575285,{"$f":"F615*(1-Elteq!$F$6)","v":36.603816291575285}]
["ANAMET-S",4650121,"DN 12","ANAFLEX hose without cover, Stainless steel AISI-316, IP 69",30,10.721016243776111,{"$f":"F616*(1-Elteq!$F$6)","v":10.721016243776111}]
["ANAMET-S",4650123,"DN 12","ANAFLEX hose without cover, Stainless steel AISI-316, IP 69",10,10.721016243776111,{"$f":"F617*(1-Elteq!$F$6)","v":10.721016243776111}]
["ANAMET-S",4650125,"DN 12","ANAFLEX hose without cover, Stainless steel AISI-316, IP 69",120,10.721016243776111,{"$f":"F618*(1-Elteq!$F$6)","v":10.721016243776111}]
["ANAMET-S",4650161,"DN 16","ANAFLEX hose without cover, Stainless steel AISI-316, IP 69",30,11.96591761003781,{"$f":"F619*(1-Elteq!$F$6)","v":11.96591761003781}]
["ANAMET-S",4650163,"DN 16","ANAFLEX hose without cover, Stainless steel AISI-316, IP 69",10,11.96591761003781,{"$f":"F620*(1-Elteq!$F$6)","v":11.96591761003781}]
["ANAMET-S",4650165,"DN 16","ANAFLEX hose without cover, Stainless steel AISI-316, IP 69",90,11.96591761003781,{"$f":"F621*(1-Elteq!$F$6)","v":11.96591761003781}]
["ANAMET-S",4650201,"DN 20","ANAFLEX hose without cover, Stainless steel AISI-316, IP 69",30,14.158430464050948,{"$f":"F622*(1-Elteq!$F$6)","v":14.158430464050948}]
["ANAMET-S",4650203,"DN 20","ANAFLEX hose without cover, Stainless steel AISI-316, IP 69",10,14.158430464050948,{"$f":"F623*(1-Elteq!$F$6)","v":14.158430464050948}]
["ANAMET-S",4650205,"DN 20","ANAFLEX hose without cover, Stainless steel AISI-316, IP 69",60,14.158430464050948,{"$f":"F624*(1-Elteq!$F$6)","v":14.158430464050948}]
["ANAMET-S",8420160,"M16 x 1,5","Multiflex fittings for  ANAFLEX, Straight fixed with male thread, IP 69K",10,4.2363807687711494,{"$f":"F625*(1-Elteq!$F$6)","v":4.2363807687711494}]
["ANAMET-S",8420170,"M20 x 1,5","Multiflex fittings for  ANAFLEX, Straight fixed with male thread, IP 69K",10,4.3292838558056053,{"$f":"F626*(1-Elteq!$F$6)","v":4.3292838558056053}]
["ANAMET-S",8420200,"M20 x 1,5","Multiflex fittings for  ANAFLEX, Straight fixed with male thread, IP 69K",10,5.9086363353913409,{"$f":"F627*(1-Elteq!$F$6)","v":5.9086363353913409}]
["ANAMET-S",8420250,"M25 x 1,5","Multiflex fittings for  ANAFLEX, Straight fixed with male thread, IP 69K",5,8.4170196853216268,{"$f":"F628*(1-Elteq!$F$6)","v":8.4170196853216268}]
["ANAMET-S",8440120,"NPT 1/2\"","Multiflex fittings for  ANAFLEX, Straight fixed with male thread, IP 69K",10,4.3292838558056053,{"$f":"F629*(1-Elteq!$F$6)","v":4.3292838558056053}]
["ANAMET-S",8440160,"NPT 1/2\"","Multiflex fittings for  ANAFLEX, Straight fixed with male thread, IP 69K",10,6.0108297311292409,{"$f":"F630*(1-Elteq!$F$6)","v":6.0108297311292409}]
["ANAMET-S",8440180,"NPT 3/4\"","Multiflex fittings for  ANAFLEX, Straight fixed with male thread, IP 69K",5,6.4474742401911795,{"$f":"F631*(1-Elteq!$F$6)","v":6.4474742401911795}]
["ANAMET-S",8440200,"NPT 3/4\"","Multiflex fittings for  ANAFLEX, Straight fixed with male thread, IP 69K",5,8.4170196853216268,{"$f":"F632*(1-Elteq!$F$6)","v":8.4170196853216268}]
["ANAMET-S",3600105,"10 mm","FCD conduit with black cover, Galvanised steel core with pvc cover",50,2.0531582234614563,{"$f":"F633*(1-Elteq!$F$6)","v":2.0531582234614563}]
["ANAMET-S",3600121,"14 mm","FCD conduit with black cover, Galvanised steel core with pvc cover",10,2.8149635371439876,{"$f":"F634*(1-Elteq!$F$6)","v":2.8149635371439876}]
["ANAMET-S",3600125,"14 mm","FCD conduit with black cover, Galvanised steel core with pvc cover",50,2.3876093367854945,{"$f":"F635*(1-Elteq!$F$6)","v":2.3876093367854945}]
["ANAMET-S",3600161,"17 mm","FCD conduit with black cover, Galvanised steel core with pvc cover",10,3.3538014419438267,{"$f":"F636*(1-Elteq!$F$6)","v":3.3538014419438267}]
["ANAMET-S",3600165,"17 mm","FCD conduit with black cover, Galvanised steel core with pvc cover",50,2.8428344632543241,{"$f":"F637*(1-Elteq!$F$6)","v":2.8428344632543241}]
["ANAMET-S",3600181,"19 mm","FCD conduit with black cover, Galvanised steel core with pvc cover",10,3.8926393467436666,{"$f":"F638*(1-Elteq!$F$6)","v":3.8926393467436666}]
["ANAMET-S",3600185,"19 mm","FCD conduit with black cover, Galvanised steel core with pvc cover",50,3.2980595897231542,{"$f":"F639*(1-Elteq!$F$6)","v":3.2980595897231542}]
["ANAMET-S",3600201,"21 mm","FCD conduit with black cover, Galvanised steel core with pvc cover",10,4.0784455208125756,{"$f":"F640*(1-Elteq!$F$6)","v":4.0784455208125756}]
["ANAMET-S",3600205,"21 mm","FCD conduit with black cover, Galvanised steel core with pvc cover",50,3.455994837681728,{"$f":"F641*(1-Elteq!$F$6)","v":3.455994837681728}]
["ANAMET-S",3600251,"27 mm","FCD conduit with black cover, Galvanised steel core with pvc cover",10,5.3419275044811645,{"$f":"F642*(1-Elteq!$F$6)","v":5.3419275044811645}]
["ANAMET-S",3600255,"27 mm","FCD conduit with black cover, Galvanised steel core with pvc cover",50,4.5243803385779611,{"$f":"F643*(1-Elteq!$F$6)","v":4.5243803385779611}]
["ANAMET-S",3600321,"36 mm","FCD conduit with black cover, Galvanised steel core with pvc cover",10,7.3300535670185027,{"$f":"F644*(1-Elteq!$F$6)","v":7.3300535670185027}]
["ANAMET-S",3600322,"36 mm","FCD conduit with black cover, Galvanised steel core with pvc cover",25,6.2152165226050426,{"$f":"F645*(1-Elteq!$F$6)","v":6.2152165226050426}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},3600401,"45 mm","FCD conduit with black cover, Galvanised steel core with pvc cover",10,12.263207488548066,{"$f":"F646*(1-Elteq!$F$6)","v":12.263207488548066}]
["ANAMET-S",3600402,"45 mm","FCD conduit with black cover, Galvanised steel core with pvc cover",25,10.39585543915552,{"$f":"F647*(1-Elteq!$F$6)","v":10.39585543915552}]
["ANAMET-S",3600501,"56 mm","FCD conduit with black cover, Galvanised steel core with pvc cover",10,15.821395721967695,{"$f":"F648*(1-Elteq!$F$6)","v":15.821395721967695}]
["ANAMET-S",3600502,"56 mm","FCD conduit with black cover, Galvanised steel core with pvc cover",25,13.405915459071862,{"$f":"F649*(1-Elteq!$F$6)","v":13.405915459071862}]
["ANAMET-S",3610105,"10 mm","FCD conduit with grey cover, Galvanised steel core with pvc cover",50,2.0531582234614563,{"$f":"F650*(1-Elteq!$F$6)","v":2.0531582234614563}]
["ANAMET-S",3610121,"14 mm","FCD conduit with grey cover, Galvanised steel core with pvc cover",10,2.8149635371439876,{"$f":"F651*(1-Elteq!$F$6)","v":2.8149635371439876}]
["ANAMET-S",3610125,"14 mm","FCD conduit with grey cover, Galvanised steel core with pvc cover",50,2.3876093367854945,{"$f":"F652*(1-Elteq!$F$6)","v":2.3876093367854945}]
["ANAMET-S",3610161,"17 mm","FCD conduit with grey cover, Galvanised steel core with pvc cover",10,3.3538014419438267,{"$f":"F653*(1-Elteq!$F$6)","v":3.3538014419438267}]
["ANAMET-S",3610165,"17 mm","FCD conduit with grey cover, Galvanised steel core with pvc cover",50,2.8428344632543241,{"$f":"F654*(1-Elteq!$F$6)","v":2.8428344632543241}]
["ANAMET-S",3610181,"19 mm","FCD conduit with grey cover, Galvanised steel core with pvc cover",10,3.8926393467436666,{"$f":"F655*(1-Elteq!$F$6)","v":3.8926393467436666}]
["ANAMET-S",3610185,"19 mm","FCD conduit with grey cover, Galvanised steel core with pvc cover",50,3.2980595897231542,{"$f":"F656*(1-Elteq!$F$6)","v":3.2980595897231542}]
["ANAMET-S",3610201,"21 mm","FCD conduit with grey cover, Galvanised steel core with pvc cover",10,4.0784455208125756,{"$f":"F657*(1-Elteq!$F$6)","v":4.0784455208125756}]
["ANAMET-S",3610205,"21 mm","FCD conduit with grey cover, Galvanised steel core with pvc cover",50,3.455994837681728,{"$f":"F658*(1-Elteq!$F$6)","v":3.455994837681728}]
["ANAMET-S",3610251,"27 mm","FCD conduit with grey cover, Galvanised steel core with pvc cover",10,5.3419275044811645,{"$f":"F659*(1-Elteq!$F$6)","v":5.3419275044811645}]
["ANAMET-S",3610255,"27 mm","FCD conduit with grey cover, Galvanised steel core with pvc cover",50,4.5243803385779611,{"$f":"F660*(1-Elteq!$F$6)","v":4.5243803385779611}]
["ANAMET-S",3610321,"36 mm","FCD conduit with grey cover, Galvanised steel core with pvc cover",10,7.3300535670185027,{"$f":"F661*(1-Elteq!$F$6)","v":7.3300535670185027}]
["ANAMET-S",3610322,"36 mm","FCD conduit with grey cover, Galvanised steel core with pvc cover",25,6.2152165226050426,{"$f":"F662*(1-Elteq!$F$6)","v":6.2152165226050426}]
["ANAMET-S",3610401,"45 mm","FCD conduit with grey cover, Galvanised steel core with pvc cover",10,12.263207488548066,{"$f":"F663*(1-Elteq!$F$6)","v":12.263207488548066}]
["ANAMET-S",3610402,"45 mm","FCD conduit with grey cover, Galvanised steel core with pvc cover",25,10.39585543915552,{"$f":"F664*(1-Elteq!$F$6)","v":10.39585543915552}]
["ANAMET-S",3610501,"56 mm","FCD conduit with grey cover, Galvanised steel core with pvc cover",10,15.821395721967695,{"$f":"F665*(1-Elteq!$F$6)","v":15.821395721967695}]
["ANAMET-S",3610502,"56 mm","FCD conduit with grey cover, Galvanised steel core with pvc cover",25,13.405915459071862,{"$f":"F666*(1-Elteq!$F$6)","v":13.405915459071862}]
["ANAMET-S",3710102,"7 mm","FCE conduit with black cover, Galvanised steel core with pvc cover",25,2.5362542760406228,{"$f":"F667*(1-Elteq!$F$6)","v":2.5362542760406228}]
["ANAMET-S",3710105,"7 mm","FCE conduit with black cover, Galvanised steel core with pvc cover",50,2.415480262895831,{"$f":"F668*(1-Elteq!$F$6)","v":2.415480262895831}]
["ANAMET-S",3710122,"10 mm","FCE conduit with black cover, Galvanised steel core with pvc cover",25,2.9357375502887795,{"$f":"F669*(1-Elteq!$F$6)","v":2.9357375502887795}]
["ANAMET-S",3710125,"10 mm","FCE conduit with black cover, Galvanised steel core with pvc cover",50,2.8056732284405421,{"$f":"F670*(1-Elteq!$F$6)","v":2.8056732284405421}]
["ANAMET-S",3710161,"13 mm","FCE conduit with black cover, Galvanised steel core with pvc cover",10,3.7904459510057658,{"$f":"F671*(1-Elteq!$F$6)","v":3.7904459510057658}]
["ANAMET-S",3710162,"13 mm","FCE conduit with black cover, Galvanised steel core with pvc cover",25,3.521026998605846,{"$f":"F672*(1-Elteq!$F$6)","v":3.521026998605846}]
["ANAMET-S",3710165,"13 mm","FCE conduit with black cover, Galvanised steel core with pvc cover",50,3.3445111332403816,{"$f":"F673*(1-Elteq!$F$6)","v":3.3445111332403816}]
["ANAMET-S",3710201,"16,9 mm","FCE conduit with black cover, Galvanised steel core with pvc cover",10,4.5615415733917422,{"$f":"F674*(1-Elteq!$F$6)","v":4.5615415733917422}]
["ANAMET-S",3710202,"16,9 mm","FCE conduit with black cover, Galvanised steel core with pvc cover",25,4.2456710774745954,{"$f":"F675*(1-Elteq!$F$6)","v":4.2456710774745954}]
["ANAMET-S",3710205,"16,9 mm","FCE conduit with black cover, Galvanised steel core with pvc cover",50,4.0691552121091306,{"$f":"F676*(1-Elteq!$F$6)","v":4.0691552121091306}]
["ANAMET-S",3710251,"21,2 mm","FCE conduit with black cover, Galvanised steel core with pvc cover",10,6.6146997968531984,{"$f":"F677*(1-Elteq!$F$6)","v":6.6146997968531984}]
["ANAMET-S",3710252,"21,2 mm","FCE conduit with black cover, Galvanised steel core with pvc cover",25,5.8436041744672229,{"$f":"F678*(1-Elteq!$F$6)","v":5.8436041744672229}]
["ANAMET-S",3710255,"21,2 mm","FCE conduit with black cover, Galvanised steel core with pvc cover",50,5.3233468870742744,{"$f":"F679*(1-Elteq!$F$6)","v":5.3233468870742744}]
["ANAMET-S",3710321,"28 mm","FCE conduit with black cover, Galvanised steel core with pvc cover",10,8.9372769727145744,{"$f":"F680*(1-Elteq!$F$6)","v":8.9372769727145744}]
["ANAMET-S",3710322,"28 mm","FCE conduit with black cover, Galvanised steel core with pvc cover",25,7.3114729496116118,{"$f":"F681*(1-Elteq!$F$6)","v":7.3114729496116118}]
["ANAMET-S",3710401,"38 mm","FCE conduit with black cover, Galvanised steel core with pvc cover",10,14.678687751443896,{"$f":"F682*(1-Elteq!$F$6)","v":14.678687751443896}]
["ANAMET-S",3710402,"38 mm","FCE conduit with black cover, Galvanised steel core with pvc cover",25,12.23533656243773,{"$f":"F683*(1-Elteq!$F$6)","v":12.23533656243773}]
["ANAMET-S",3710501,"48 mm","FCE conduit with black cover, Galvanised steel core with pvc cover",10,18.366940306711761,{"$f":"F684*(1-Elteq!$F$6)","v":18.366940306711761}]
["ANAMET-S",3710502,"48 mm","FCE conduit with black cover, Galvanised steel core with pvc cover",25,15.774944178450465,{"$f":"F685*(1-Elteq!$F$6)","v":15.774944178450465}]
["ANAMET-S",3720125,"10 mm","FCE conduit with grey cover, Galvanised steel core with pvc cover",50,2.8056732284405421,{"$f":"F686*(1-Elteq!$F$6)","v":2.8056732284405421}]
["ANAMET-S",3720161,"13 mm","FCE conduit with grey cover, Galvanised steel core with pvc cover",10,3.7904459510057658,{"$f":"F687*(1-Elteq!$F$6)","v":3.7904459510057658}]
["ANAMET-S",3720165,"13 mm","FCE conduit with grey cover, Galvanised steel core with pvc cover",50,3.3445111332403816,{"$f":"F688*(1-Elteq!$F$6)","v":3.3445111332403816}]
["ANAMET-S",3720201,"16,9 mm","FCE conduit with grey cover, Galvanised steel core with pvc cover",10,4.5615415733917422,{"$f":"F689*(1-Elteq!$F$6)","v":4.5615415733917422}]
["ANAMET-S",3720205,"16,9 mm","FCE conduit with grey cover, Galvanised steel core with pvc cover",50,4.0691552121091306,{"$f":"F690*(1-Elteq!$F$6)","v":4.0691552121091306}]
["ANAMET-S",3720251,"21,2 mm","FCE conduit with grey cover, Galvanised steel core with pvc cover",10,6.6146997968531984,{"$f":"F691*(1-Elteq!$F$6)","v":6.6146997968531984}]
["ANAMET-S",3720255,"21,2 mm","FCE conduit with grey cover, Galvanised steel core with pvc cover",50,5.3233468870742744,{"$f":"F692*(1-Elteq!$F$6)","v":5.3233468870742744}]
["ANAMET-S",3720321,"28 mm","FCE conduit with grey cover, Galvanised steel core with pvc cover",10,8.9372769727145744,{"$f":"F693*(1-Elteq!$F$6)","v":8.9372769727145744}]
["ANAMET-S",3720322,"28 mm","FCE conduit with grey cover, Galvanised steel core with pvc cover",25,7.3114729496116118,{"$f":"F694*(1-Elteq!$F$6)","v":7.3114729496116118}]
["ANAMET-S",3720401,"38 mm","FCE conduit with grey cover, Galvanised steel core with pvc cover",10,14.678687751443896,{"$f":"F695*(1-Elteq!$F$6)","v":14.678687751443896}]
["ANAMET-S",3720501,"48 mm","FCE conduit with grey cover, Galvanised steel core with pvc cover",10,18.366940306711761,{"$f":"F696*(1-Elteq!$F$6)","v":18.366940306711761}]
["ANAMET-S",3730122,"10 mm","FCE-LFH conduit with black cover, Galvanised steel core, Polyolefin cover",25,3.2516080462059263,{"$f":"F697*(1-Elteq!$F$6)","v":3.2516080462059263}]
["ANAMET-S",3730162,"13 mm","FCE-LFH conduit with black cover, Galvanised steel core, Polyolefin cover",25,4.1156067556263585,{"$f":"F698*(1-Elteq!$F$6)","v":4.1156067556263585}]
["ANAMET-S",3730165,"13 mm","FCE-LFH conduit with black cover, Galvanised steel core, Polyolefin cover",50,4.0134133598884576,{"$f":"F699*(1-Elteq!$F$6)","v":4.0134133598884576}]
["ANAMET-S",3730201,"16,9 mm","FCE-LFH conduit with black cover, Galvanised steel core, Polyolefin cover",10,4.9981860824536808,{"$f":"F700*(1-Elteq!$F$6)","v":4.9981860824536808}]
["ANAMET-S",3730202,"16,9 mm","FCE-LFH conduit with black cover, Galvanised steel core, Polyolefin cover",25,4.8495411431985529,{"$f":"F701*(1-Elteq!$F$6)","v":4.8495411431985529}]
["ANAMET-S",3730205,"16,9 mm","FCE-LFH conduit with black cover, Galvanised steel core, Polyolefin cover",50,4.663734969129643,{"$f":"F702*(1-Elteq!$F$6)","v":4.663734969129643}]
["ANAMET-S",3730251,"21,2 mm","FCE-LFH conduit with black cover, Galvanised steel core, Polyolefin cover",10,7.0513443059151371,{"$f":"F703*(1-Elteq!$F$6)","v":7.0513443059151371}]
["ANAMET-S",3730252,"21,2 mm","FCE-LFH conduit with black cover, Galvanised steel core, Polyolefin cover",25,6.7912156622186624,{"$f":"F704*(1-Elteq!$F$6)","v":6.7912156622186624}]
["ANAMET-S",3730255,"21,2 mm","FCE-LFH conduit with black cover, Galvanised steel core, Polyolefin cover",50,6.5496676359290804,{"$f":"F705*(1-Elteq!$F$6)","v":6.5496676359290804}]
["ANAMET-S",3730321,"28 mm","FCE-LFH conduit with black cover, Galvanised steel core, Polyolefin cover",10,11.362047544313851,{"$f":"F706*(1-Elteq!$F$6)","v":11.362047544313851}]
["ANAMET-S",3730322,"28 mm","FCE-LFH conduit with black cover, Galvanised steel core, Polyolefin cover",25,10.971854578769141,{"$f":"F707*(1-Elteq!$F$6)","v":10.971854578769141}]
["ANAMET-S",3730401,"38 mm","FCE-LFH conduit with black cover, Galvanised steel core, Polyolefin cover",10,18.46913370244966,{"$f":"F708*(1-Elteq!$F$6)","v":18.46913370244966}]
["ANAMET-S",3730402,"38 mm","FCE-LFH conduit with black cover, Galvanised steel core, Polyolefin cover",25,17.828102401911924,{"$f":"F709*(1-Elteq!$F$6)","v":17.828102401911924}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},3730501,"48 mm","FCE-LFH conduit with black cover, Galvanised steel core, Polyolefin cover",10,23.783190280820492,{"$f":"F710*(1-Elteq!$F$6)","v":23.783190280820492}]
["ANAMET-S",3730502,"48 mm","FCE-LFH conduit with black cover, Galvanised steel core, Polyolefin cover",25,22.95635280621384,{"$f":"F711*(1-Elteq!$F$6)","v":22.95635280621384}]
["ANAMET-S",3740122,"10 mm","FCE-PUV0 conduit with black cover, Galvanised steel core with TPU cover",25,6.5125064011152984,{"$f":"F712*(1-Elteq!$F$6)","v":6.5125064011152984}]
["ANAMET-S",3740162,"13 mm","FCE-PUV0 conduit with black cover, Galvanised steel core with TPU cover",25,8.2219232025492701,{"$f":"F713*(1-Elteq!$F$6)","v":8.2219232025492701}]
["ANAMET-S",3740202,"16,9 mm","FCE-PUV0 conduit with black cover, Galvanised steel core with TPU cover",25,9.6990822863971058,{"$f":"F714*(1-Elteq!$F$6)","v":9.6990822863971058}]
["ANAMET-S",3740252,"21,2 mm","FCE-PUV0 conduit with black cover, Galvanised steel core with TPU cover",25,13.573141015733881,{"$f":"F715*(1-Elteq!$F$6)","v":13.573141015733881}]
["ANAMET-S",3740322,"28 mm","FCE-PUV0 conduit with black cover, Galvanised steel core with TPU cover",25,21.943709157538283,{"$f":"F716*(1-Elteq!$F$6)","v":21.943709157538283}]
["ANAMET-S",3740401,"38 mm","FCE-PUV0 conduit with black cover, Galvanised steel core with TPU cover",10,36.94755771360277,{"$f":"F717*(1-Elteq!$F$6)","v":36.94755771360277}]
["ANAMET-S",3740501,"48 mm","FCE-PUV0 conduit with black cover, Galvanised steel core with TPU cover",10,47.575670870344425,{"$f":"F718*(1-Elteq!$F$6)","v":47.575670870344425}]
["ANAMET-S",2601100,"M10 X 1,0","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",10,1.7187071101374183,{"$f":"F719*(1-Elteq!$F$6)","v":1.7187071101374183}]
["ANAMET-S",2601110,"M12 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",10,1.9881260625373383,{"$f":"F720*(1-Elteq!$F$6)","v":1.9881260625373383}]
["ANAMET-S",2601120,"M12 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",10,1.9881260625373383,{"$f":"F721*(1-Elteq!$F$6)","v":1.9881260625373383}]
["ANAMET-S",2601150,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",10,1.9881260625373383,{"$f":"F722*(1-Elteq!$F$6)","v":1.9881260625373383}]
["ANAMET-S",2601160,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",10,2.2761256323441486,{"$f":"F723*(1-Elteq!$F$6)","v":2.2761256323441486}]
["ANAMET-S",2601170,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",10,2.4805124238199494,{"$f":"F724*(1-Elteq!$F$6)","v":2.4805124238199494}]
["ANAMET-S",2601180,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",10,2.9636084763991155,{"$f":"F725*(1-Elteq!$F$6)","v":2.9636084763991155}]
["ANAMET-S",2601200,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",10,2.9636084763991155,{"$f":"F726*(1-Elteq!$F$6)","v":2.9636084763991155}]
["ANAMET-S",2601250,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",5,4.3107032383987134,{"$f":"F727*(1-Elteq!$F$6)","v":4.3107032383987134}]
["ANAMET-S",2601320,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",5,7.5065694323839676,{"$f":"F728*(1-Elteq!$F$6)","v":7.5065694323839676}]
["ANAMET-S",2601400,"M40 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",2,12.616239219278995,{"$f":"F729*(1-Elteq!$F$6)","v":12.616239219278995}]
["ANAMET-S",2601500,"M50 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",2,22.064483170683072,{"$f":"F730*(1-Elteq!$F$6)","v":22.064483170683072}]
["ANAMET-S",2601600,"M63 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",2,31.56846897430782,{"$f":"F731*(1-Elteq!$F$6)","v":31.56846897430782}]
["ANAMET-S",2602070,"PG 7","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",10,1.9230939016132194,{"$f":"F732*(1-Elteq!$F$6)","v":1.9230939016132194}]
["ANAMET-S",2602090,"PG 9","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",10,2.1925128540131387,{"$f":"F733*(1-Elteq!$F$6)","v":2.1925128540131387}]
["ANAMET-S",2602110,"PG 11","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",10,2.378319028082049,{"$f":"F734*(1-Elteq!$F$6)","v":2.378319028082049}]
["ANAMET-S",2602130,"PG 13,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",10,2.926447241585334,{"$f":"F735*(1-Elteq!$F$6)","v":2.926447241585334}]
["ANAMET-S",2602160,"PG 16","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",10,3.028640637323234,{"$f":"F736*(1-Elteq!$F$6)","v":3.028640637323234}]
["ANAMET-S",2602210,"PG 21","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",5,4.4036063254331692,{"$f":"F737*(1-Elteq!$F$6)","v":4.4036063254331692}]
["ANAMET-S",2602290,"PG 29","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",5,8.3055359808802809,{"$f":"F738*(1-Elteq!$F$6)","v":8.3055359808802809}]
["ANAMET-S",2602360,"PG 36","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",2,13.517399163513209,{"$f":"F739*(1-Elteq!$F$6)","v":13.517399163513209}]
["ANAMET-S",2602480,"PG 48","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 54",2,31.56846897430782,{"$f":"F740*(1-Elteq!$F$6)","v":31.56846897430782}]
["ANAMET-S",2603110,"M12 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 54",10,2.322577175861376,{"$f":"F741*(1-Elteq!$F$6)","v":2.322577175861376}]
["ANAMET-S",2603120,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 54",10,2.4712221151165039,{"$f":"F742*(1-Elteq!$F$6)","v":2.4712221151165039}]
["ANAMET-S",2603160,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 54",10,2.4712221151165039,{"$f":"F743*(1-Elteq!$F$6)","v":2.4712221151165039}]
["ANAMET-S",2603170,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 54",10,2.7034798327026417,{"$f":"F744*(1-Elteq!$F$6)","v":2.7034798327026417}]
["ANAMET-S",2603200,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 54",10,3.1679952678749173,{"$f":"F745*(1-Elteq!$F$6)","v":3.1679952678749173}]
["ANAMET-S",2603250,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 54",5,5.2304438000398186,{"$f":"F746*(1-Elteq!$F$6)","v":5.2304438000398186}]
["ANAMET-S",2603320,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 54",5,9.188115307707605,{"$f":"F747*(1-Elteq!$F$6)","v":9.188115307707605}]
["ANAMET-S",2603400,"M40 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 54",2,11.882304831706799,{"$f":"F748*(1-Elteq!$F$6)","v":11.882304831706799}]
["ANAMET-S",2603500,"M50 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 54",2,19.40745488149766,{"$f":"F749*(1-Elteq!$F$6)","v":19.40745488149766}]
["ANAMET-S",2611100,"M10 x 1,0","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",10,2.5548348934475134,{"$f":"F750*(1-Elteq!$F$6)","v":2.5548348934475134}]
["ANAMET-S",2611110,"M12 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",10,2.5548348934475134,{"$f":"F751*(1-Elteq!$F$6)","v":2.5548348934475134}]
["ANAMET-S",2611120,"M12 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",10,2.5548348934475134,{"$f":"F752*(1-Elteq!$F$6)","v":2.5548348934475134}]
["ANAMET-S",2611150,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",10,2.6756089065923048,{"$f":"F753*(1-Elteq!$F$6)","v":2.6756089065923048}]
["ANAMET-S",2611160,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",10,2.6848992152957507,{"$f":"F754*(1-Elteq!$F$6)","v":2.6848992152957507}]
["ANAMET-S",2611170,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",10,3.0565115634335709,{"$f":"F755*(1-Elteq!$F$6)","v":3.0565115634335709}]
["ANAMET-S",2611180,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",10,3.6510913204540834,{"$f":"F756*(1-Elteq!$F$6)","v":3.6510913204540834}]
["ANAMET-S",2611200,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",10,3.6789622465644194,{"$f":"F757*(1-Elteq!$F$6)","v":3.6789622465644194}]
["ANAMET-S",2611250,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",5,5.5184433698466293,{"$f":"F758*(1-Elteq!$F$6)","v":5.5184433698466293}]
["ANAMET-S",2611320,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",5,9.7641144473212247,{"$f":"F759*(1-Elteq!$F$6)","v":9.7641144473212247}]
["ANAMET-S",2611400,"M40 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",2,16.40668517028476,{"$f":"F760*(1-Elteq!$F$6)","v":16.40668517028476}]
["ANAMET-S",2611500,"M50 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",2,37.309879753037144,{"$f":"F761*(1-Elteq!$F$6)","v":37.309879753037144}]
["ANAMET-S",2611600,"M63 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",2,41.044583851822239,{"$f":"F762*(1-Elteq!$F$6)","v":41.044583851822239}]
["ANAMET-S",2612070,"PG 7","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",10,2.7499313762198692,{"$f":"F763*(1-Elteq!$F$6)","v":2.7499313762198692}]
["ANAMET-S",2612090,"PG 9","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",10,2.7778023023302061,{"$f":"F764*(1-Elteq!$F$6)","v":2.7778023023302061}]
["ANAMET-S",2612110,"PG 11","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",10,2.8985763154749975,{"$f":"F765*(1-Elteq!$F$6)","v":2.8985763154749975}]
["ANAMET-S",2612130,"PG 13,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",10,3.5117366899024001,{"$f":"F766*(1-Elteq!$F$6)","v":3.5117366899024001}]
["ANAMET-S",2612160,"PG 16","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",10,3.6325107030471924,{"$f":"F767*(1-Elteq!$F$6)","v":3.6325107030471924}]
["ANAMET-S",2612210,"PG 21","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",5,6.1037328181636967,{"$f":"F768*(1-Elteq!$F$6)","v":6.1037328181636967}]
["ANAMET-S",2612290,"PG 29","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",5,10.804629022107122,{"$f":"F769*(1-Elteq!$F$6)","v":10.804629022107122}]
["ANAMET-S",2612360,"PG 36","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",2,17.577264066918893,{"$f":"F770*(1-Elteq!$F$6)","v":17.577264066918893}]
["ANAMET-S",2612480,"PG 48","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 54",2,41.044583851822239,{"$f":"F771*(1-Elteq!$F$6)","v":41.044583851822239}]
["ANAMET-S",2622100,"- ","Multiflex fittings for FCE / FCD, Straight fixed box connector, IP 54",10,1.3470947619995981,{"$f":"F772*(1-Elteq!$F$6)","v":1.3470947619995981}]
["ANAMET-S",2622120,"- ","Multiflex fittings for FCE / FCD, Straight fixed box connector, IP 54",10,1.4585784664409442,{"$f":"F773*(1-Elteq!$F$6)","v":1.4585784664409442}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},2622160,"- ","Multiflex fittings for FCE / FCD, Straight fixed box connector, IP 54",10,1.8766423580959919,{"$f":"F774*(1-Elteq!$F$6)","v":1.8766423580959919}]
["ANAMET-S",2622180,"- ","Multiflex fittings for FCE / FCD, Straight fixed box connector, IP 54",10,1.9138035929097739,{"$f":"F775*(1-Elteq!$F$6)","v":1.9138035929097739}]
["ANAMET-S",2622200,"- ","Multiflex fittings for FCE / FCD, Straight fixed box connector, IP 54",5,2.0067066799442288,{"$f":"F776*(1-Elteq!$F$6)","v":2.0067066799442288}]
["ANAMET-S",2622250,"- ","Multiflex fittings for FCE / FCD, Straight fixed box connector, IP 54",5,2.8149635371439876,{"$f":"F777*(1-Elteq!$F$6)","v":2.8149635371439876}]
["ANAMET-S",2622320,"- ","Multiflex fittings for FCE / FCD, Straight fixed box connector, IP 54",5,4.2270904600677044,{"$f":"F778*(1-Elteq!$F$6)","v":4.2270904600677044}]
["ANAMET-S",2622400,"- ","Multiflex fittings for FCE / FCD, Straight fixed box connector, IP 54",2,7.952504250149353,{"$f":"F779*(1-Elteq!$F$6)","v":7.952504250149353}]
["ANAMET-S",2622500,"- ","Multiflex fittings for FCE / FCD, Straight fixed box connector, IP 54",2,19.649002907787242,{"$f":"F780*(1-Elteq!$F$6)","v":19.649002907787242}]
["ANAMET-S",2641100,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",10,1.2170304401513612,{"$f":"F781*(1-Elteq!$F$6)","v":1.2170304401513612}]
["ANAMET-S",2641120,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",10,1.2727722923720342,{"$f":"F782*(1-Elteq!$F$6)","v":1.2727722923720342}]
["ANAMET-S",2641160,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",10,1.5886427882891812,{"$f":"F783*(1-Elteq!$F$6)","v":1.5886427882891812}]
["ANAMET-S",2641180,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",10,1.5886427882891812,{"$f":"F784*(1-Elteq!$F$6)","v":1.5886427882891812}]
["ANAMET-S",2641200,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",10,1.969545445130447,{"$f":"F785*(1-Elteq!$F$6)","v":1.969545445130447}]
["ANAMET-S",2641250,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",5,2.7406410675164237,{"$f":"F786*(1-Elteq!$F$6)","v":2.7406410675164237}]
["ANAMET-S",2641320,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",5,4.0784455208125756,{"$f":"F787*(1-Elteq!$F$6)","v":4.0784455208125756}]
["ANAMET-S",2641400,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",2,7.8317302370045585,{"$f":"F788*(1-Elteq!$F$6)","v":7.8317302370045585}]
["ANAMET-S",2641500,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",2,12.095981931886046,{"$f":"F789*(1-Elteq!$F$6)","v":12.095981931886046}]
["ANAMET-S",7120144,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",10,3.9762521250746765,{"$f":"F790*(1-Elteq!$F$6)","v":3.9762521250746765}]
["ANAMET-S",7120154,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",10,3.7254137900816469,{"$f":"F791*(1-Elteq!$F$6)","v":3.7254137900816469}]
["ANAMET-S",7120164,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",10,2.7963829197370966,{"$f":"F792*(1-Elteq!$F$6)","v":2.7963829197370966}]
["ANAMET-S",7120174,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",10,3.047221254730125,{"$f":"F793*(1-Elteq!$F$6)","v":3.047221254730125}]
["ANAMET-S",7120204,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",10,3.2237371200955898,{"$f":"F794*(1-Elteq!$F$6)","v":3.2237371200955898}]
["ANAMET-S",7120254,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",5,4.9981860824536808,{"$f":"F795*(1-Elteq!$F$6)","v":4.9981860824536808}]
["ANAMET-S",7120324,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",5,7.9617945588527972,{"$f":"F796*(1-Elteq!$F$6)","v":7.9617945588527972}]
["ANAMET-S",7120404,"M40 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",2,14.790171455885242,{"$f":"F797*(1-Elteq!$F$6)","v":14.790171455885242}]
["ANAMET-S",7120454,"M50 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",1,23.978286763592848,{"$f":"F798*(1-Elteq!$F$6)","v":23.978286763592848}]
["ANAMET-S",7120554,"M50 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",1,25.947832208723295,{"$f":"F799*(1-Elteq!$F$6)","v":25.947832208723295}]
["ANAMET-S",7120604,"M63 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",1,40.096972364070794,{"$f":"F800*(1-Elteq!$F$6)","v":40.096972364070794}]
["ANAMET-S",7129144,"M20 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",10,6.8376672057358912,{"$f":"F801*(1-Elteq!$F$6)","v":6.8376672057358912}]
["ANAMET-S",7129154,"M16 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",10,5.9550878789085679,{"$f":"F802*(1-Elteq!$F$6)","v":5.9550878789085679}]
["ANAMET-S",7129164,"M16 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",10,5.0260570085640177,{"$f":"F803*(1-Elteq!$F$6)","v":5.0260570085640177}]
["ANAMET-S",7129174,"M20 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",10,5.9086363353913409,{"$f":"F804*(1-Elteq!$F$6)","v":5.9086363353913409}]
["ANAMET-S",7129204,"M20 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",10,5.9922491137223508,{"$f":"F805*(1-Elteq!$F$6)","v":5.9922491137223508}]
["ANAMET-S",7129254,"M25 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",5,9.4761148775144139,{"$f":"F806*(1-Elteq!$F$6)","v":9.4761148775144139}]
["ANAMET-S",7129324,"M32 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",5,17.252103262298302,{"$f":"F807*(1-Elteq!$F$6)","v":17.252103262298302}]
["ANAMET-S",7129454,"M50 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",2,41.955034104759889,{"$f":"F808*(1-Elteq!$F$6)","v":41.955034104759889}]
["ANAMET-S",7129554,"M50 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",2,43.813095845448991,{"$f":"F809*(1-Elteq!$F$6)","v":43.813095845448991}]
["ANAMET-S",7129604,"M63 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",2,68.088672487552103,{"$f":"F810*(1-Elteq!$F$6)","v":68.088672487552103}]
["ANAMET-S",7830160,"M 16 x 1,5","Multiflex fittings for FCE / FCD, Elbow fitting male/female",10,3.0100600199163439,{"$f":"F811*(1-Elteq!$F$6)","v":3.0100600199163439}]
["ANAMET-S",7830200,"M 20 x 1,5","Multiflex fittings for FCE / FCD, Elbow fitting male/female",10,3.455994837681728,{"$f":"F812*(1-Elteq!$F$6)","v":3.455994837681728}]
["ANAMET-S",7830250,"M 25 x 1,5","Multiflex fittings for FCE / FCD, Elbow fitting male/female",5,7.1163764668392568,{"$f":"F813*(1-Elteq!$F$6)","v":7.1163764668392568}]
["ANAMET-S",7830320,"M 32 x 1,5","Multiflex fittings for FCE / FCD, Elbow fitting male/female",5,11.947336992630918,{"$f":"F814*(1-Elteq!$F$6)","v":11.947336992630918}]
["ANAMET-S",8130154,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 65",10,7.1814086277633749,{"$f":"F815*(1-Elteq!$F$6)","v":7.1814086277633749}]
["ANAMET-S",8130164,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 65",10,6.5589579446325255,{"$f":"F816*(1-Elteq!$F$6)","v":6.5589579446325255}]
["ANAMET-S",8130204,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 65",10,7.4508275801632937,{"$f":"F817*(1-Elteq!$F$6)","v":7.4508275801632937}]
["ANAMET-S",8130254,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 65",5,9.8105659908384535,{"$f":"F818*(1-Elteq!$F$6)","v":9.8105659908384535}]
["ANAMET-S",8130324,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 65",5,16.323072391953751,{"$f":"F819*(1-Elteq!$F$6)","v":16.323072391953751}]
["ANAMET-S",8130454,"M50 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 65",2,37.858007966540427,{"$f":"F820*(1-Elteq!$F$6)","v":37.858007966540427}]
["ANAMET-S",8130554,"M50 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 65",2,39.716069707229529,{"$f":"F821*(1-Elteq!$F$6)","v":39.716069707229529}]
["ANAMET-S",8130604,"M63 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 65",2,61.5761660864368,{"$f":"F822*(1-Elteq!$F$6)","v":61.5761660864368}]
["ANAMET-S",7100114,"PG 11","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",10,2.8428344632543241,{"$f":"F823*(1-Elteq!$F$6)","v":2.8428344632543241}]
["ANAMET-S",7100134,"PG 13,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",10,2.8521247719577696,{"$f":"F824*(1-Elteq!$F$6)","v":2.8521247719577696}]
["ANAMET-S",7100164,"PG 16","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",10,3.3630917506472726,{"$f":"F825*(1-Elteq!$F$6)","v":3.3630917506472726}]
["ANAMET-S",7100214,"PG 21","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",5,5.1003794781915825,{"$f":"F826*(1-Elteq!$F$6)","v":5.1003794781915825}]
["ANAMET-S",7100294,"PG 29","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",5,8.3055359808802809,{"$f":"F827*(1-Elteq!$F$6)","v":8.3055359808802809}]
["ANAMET-S",7100404,"PG 42","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",2,22.58474045807602,{"$f":"F828*(1-Elteq!$F$6)","v":22.58474045807602}]
["ANAMET-S",7100454,"PG 42","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",2,24.442802198765119,{"$f":"F829*(1-Elteq!$F$6)","v":24.442802198765119}]
["ANAMET-S",7100504,"PG 48","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",2,37.727943644692189,{"$f":"F830*(1-Elteq!$F$6)","v":37.727943644692189}]
["ANAMET-S",7109114,"PG 11","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65","-",5.2304438000398186,{"$f":"F831*(1-Elteq!$F$6)","v":5.2304438000398186}]
["ANAMET-S",7109134,"PG 13,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65","-",5.3976693567018375,{"$f":"F832*(1-Elteq!$F$6)","v":5.3976693567018375}]
["ANAMET-S",7109164,"PG 16","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65","-",6.3917323879705075,{"$f":"F833*(1-Elteq!$F$6)","v":6.3917323879705075}]
["ANAMET-S",7109214,"PG 21","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65","-",9.364631173073068,{"$f":"F834*(1-Elteq!$F$6)","v":9.364631173073068}]
["ANAMET-S",7109294,"PG 29","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65","-",17.493651288587884,{"$f":"F835*(1-Elteq!$F$6)","v":17.493651288587884}]
["ANAMET-S",7109404,"PG 42","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",2,41.955034104759889,{"$f":"F836*(1-Elteq!$F$6)","v":41.955034104759889}]
["ANAMET-S",7109454,"PG 42","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",2,43.813095845448991,{"$f":"F837*(1-Elteq!$F$6)","v":43.813095845448991}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},7109504,"PG 48","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",2,70.206862871937673,{"$f":"F838*(1-Elteq!$F$6)","v":70.206862871937673}]
["ANAMET-S",7140124,"NPT 1/2\"","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",10,3.465285146385173,{"$f":"F839*(1-Elteq!$F$6)","v":3.465285146385173}]
["ANAMET-S",7140164,"NPT 1/2\"","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",10,3.8926393467436666,{"$f":"F840*(1-Elteq!$F$6)","v":3.8926393467436666}]
["ANAMET-S",7140204,"NPT 3/4\"","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",5,5.3883790479983924,{"$f":"F841*(1-Elteq!$F$6)","v":5.3883790479983924}]
["ANAMET-S",7140264,"NPT 1\"","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",5,9.4389536427006338,{"$f":"F842*(1-Elteq!$F$6)","v":9.4389536427006338}]
["ANAMET-S",7140354,"NPT 1.1/2\"","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",2,24.015447998406628,{"$f":"F843*(1-Elteq!$F$6)","v":24.015447998406628}]
["ANAMET-S",7140454,"NPT 1.1/2\"","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",2,25.873509739095731,{"$f":"F844*(1-Elteq!$F$6)","v":25.873509739095731}]
["ANAMET-S",7140554,"NPT 2\"","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 65",2,44.435546528579842,{"$f":"F845*(1-Elteq!$F$6)","v":44.435546528579842}]
["ANAMET-S",7149124,"NPT 1/2\"","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",10,5.4719918263294023,{"$f":"F846*(1-Elteq!$F$6)","v":5.4719918263294023}]
["ANAMET-S",7149164,"NPT 1/2\"","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",10,6.5125064011152984,{"$f":"F847*(1-Elteq!$F$6)","v":6.5125064011152984}]
["ANAMET-S",7149204,"NPT 3/4\"","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",5,9.3088893208523942,{"$f":"F848*(1-Elteq!$F$6)","v":9.3088893208523942}]
["ANAMET-S",7149264,"NPT 1\"","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",5,17.252103262298302,{"$f":"F849*(1-Elteq!$F$6)","v":17.252103262298302}]
["ANAMET-S",7149354,"NPT 1.1/2\"","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",2,41.955034104759889,{"$f":"F850*(1-Elteq!$F$6)","v":41.955034104759889}]
["ANAMET-S",7149454,"NPT 1.1/2\"","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",2,43.813095845448991,{"$f":"F851*(1-Elteq!$F$6)","v":43.813095845448991}]
["ANAMET-S",7149554,"NPT 2\"","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 65",2,68.088672487552103,{"$f":"F852*(1-Elteq!$F$6)","v":68.088672487552103}]
["ANAMET-S",8127164,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",10,10.024243091017699,{"$f":"F853*(1-Elteq!$F$6)","v":10.024243091017699}]
["ANAMET-S",8127174,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",10,10.135726795459044,{"$f":"F854*(1-Elteq!$F$6)","v":10.135726795459044}]
["ANAMET-S",8127204,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",10,12.356110575582521,{"$f":"F855*(1-Elteq!$F$6)","v":12.356110575582521}]
["ANAMET-S",8127224,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",10,15.403331830312645,{"$f":"F856*(1-Elteq!$F$6)","v":15.403331830312645}]
["ANAMET-S",8127254,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",5,19.305261485759761,{"$f":"F857*(1-Elteq!$F$6)","v":19.305261485759761}]
["ANAMET-S",8127284,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",5,21.358419709221213,{"$f":"F858*(1-Elteq!$F$6)","v":21.358419709221213}]
["ANAMET-S",8127324,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",5,49.23863612826117,{"$f":"F859*(1-Elteq!$F$6)","v":49.23863612826117}]
["ANAMET-S",8127454,"M50 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",2,98.012756821350067,{"$f":"F860*(1-Elteq!$F$6)","v":98.012756821350067}]
["ANAMET-S",8127554,"M50 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",2,99.870818562039176,{"$f":"F861*(1-Elteq!$F$6)","v":99.870818562039176}]
["ANAMET-S",8127604,"M63 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",2,152.63977199760964,{"$f":"F862*(1-Elteq!$F$6)","v":152.63977199760964}]
["ANAMET-S",8139154,"M16 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 65",10,13.062174037044379,{"$f":"F863*(1-Elteq!$F$6)","v":13.062174037044379}]
["ANAMET-S",8139164,"M16 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 65",10,11.519982792272426,{"$f":"F864*(1-Elteq!$F$6)","v":11.519982792272426}]
["ANAMET-S",8139204,"M20 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 65",10,14.920235777733479,{"$f":"F865*(1-Elteq!$F$6)","v":14.920235777733479}]
["ANAMET-S",8139254,"M25 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 65",5,23.959706146185955,{"$f":"F866*(1-Elteq!$F$6)","v":23.959706146185955}]
["ANAMET-S",8139324,"M32 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 65",5,38.573361736705735,{"$f":"F867*(1-Elteq!$F$6)","v":38.573361736705735}]
["ANAMET-S",2641100,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",10,1.2170304401513612,{"$f":"F868*(1-Elteq!$F$6)","v":1.2170304401513612}]
["ANAMET-S",2641120,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",10,1.2727722923720342,{"$f":"F869*(1-Elteq!$F$6)","v":1.2727722923720342}]
["ANAMET-S",2641160,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",10,1.5886427882891812,{"$f":"F870*(1-Elteq!$F$6)","v":1.5886427882891812}]
["ANAMET-S",2641180,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",10,1.5886427882891812,{"$f":"F871*(1-Elteq!$F$6)","v":1.5886427882891812}]
["ANAMET-S",2641200,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",10,1.969545445130447,{"$f":"F872*(1-Elteq!$F$6)","v":1.969545445130447}]
["ANAMET-S",2641250,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",5,2.7406410675164237,{"$f":"F873*(1-Elteq!$F$6)","v":2.7406410675164237}]
["ANAMET-S",2641320,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",5,4.0784455208125756,{"$f":"F874*(1-Elteq!$F$6)","v":4.0784455208125756}]
["ANAMET-S",2641400,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",2,7.8317302370045585,{"$f":"F875*(1-Elteq!$F$6)","v":7.8317302370045585}]
["ANAMET-S",2641500,"-","Multiflex fittings for FCE / FCD, End cap, IP 54",2,12.095981931886046,{"$f":"F876*(1-Elteq!$F$6)","v":12.095981931886046}]
["ANAMET-S",7120165,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",10,3.3538014419438267,{"$f":"F877*(1-Elteq!$F$6)","v":3.3538014419438267}]
["ANAMET-S",7120175,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",10,3.6603816291575288,{"$f":"F878*(1-Elteq!$F$6)","v":3.6603816291575288}]
["ANAMET-S",7120205,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",10,3.8647684206333297,{"$f":"F879*(1-Elteq!$F$6)","v":3.8647684206333297}]
["ANAMET-S",7120255,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",5,6.0015394224257959,{"$f":"F880*(1-Elteq!$F$6)","v":6.0015394224257959}]
["ANAMET-S",7120325,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",5,9.5504373471419779,{"$f":"F881*(1-Elteq!$F$6)","v":9.5504373471419779}]
["ANAMET-S",7120405,"M40 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",2,18.199714750049743,{"$f":"F882*(1-Elteq!$F$6)","v":18.199714750049743}]
["ANAMET-S",7129165,"M16 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",10,6.0294103485361328,{"$f":"F883*(1-Elteq!$F$6)","v":6.0294103485361328}]
["ANAMET-S",7129175,"M20 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",10,7.0885055407289199,{"$f":"F884*(1-Elteq!$F$6)","v":7.0885055407289199}]
["ANAMET-S",7129205,"M20 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",10,7.1906989364668199,{"$f":"F885*(1-Elteq!$F$6)","v":7.1906989364668199}]
["ANAMET-S",7129255,"M25 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",5,11.371337853017296,{"$f":"F886*(1-Elteq!$F$6)","v":11.371337853017296}]
["ANAMET-S",7129325,"M32 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",5,20.698807791276582,{"$f":"F887*(1-Elteq!$F$6)","v":20.698807791276582}]
["ANAMET-S",7840104,"-","Multiflex fittings for FCE / FCD, Conduit connector, IP 65",10,6.0851522007568049,{"$f":"F888*(1-Elteq!$F$6)","v":6.0851522007568049}]
["ANAMET-S",7840124,"-","Multiflex fittings for FCE / FCD, Conduit connector, IP 65",10,5.1561213304122546,{"$f":"F889*(1-Elteq!$F$6)","v":5.1561213304122546}]
["ANAMET-S",7840164,"-","Multiflex fittings for FCE / FCD, Conduit connector, IP 65",10,6.2709583748257147,{"$f":"F890*(1-Elteq!$F$6)","v":6.2709583748257147}]
["ANAMET-S",7840204,"-","Multiflex fittings for FCE / FCD, Conduit connector, IP 65",5,9.4296633339971869,{"$f":"F891*(1-Elteq!$F$6)","v":9.4296633339971869}]
["ANAMET-S",7840264,"-","Multiflex fittings for FCE / FCD, Conduit connector, IP 65",5,16.917652148974263,{"$f":"F892*(1-Elteq!$F$6)","v":16.917652148974263}]
["ANAMET-S",7840354,"-","Multiflex fittings for FCE / FCD, Conduit connector, IP 65",2,38.090265684126571,{"$f":"F893*(1-Elteq!$F$6)","v":38.090265684126571}]
["ANAMET-S",7840454,"-","Multiflex fittings for FCE / FCD, Conduit connector, IP 65",2,56.949592352120938,{"$f":"F894*(1-Elteq!$F$6)","v":56.949592352120938}]
["ANAMET-S",8120125,"M12 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",10,4.3664450906193863,{"$f":"F895*(1-Elteq!$F$6)","v":4.3664450906193863}]
["ANAMET-S",8130165,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 68",10,7.8688914718183423,{"$f":"F896*(1-Elteq!$F$6)","v":7.8688914718183423}]
["ANAMET-S",8130205,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 68",10,8.9372769727145744,{"$f":"F897*(1-Elteq!$F$6)","v":8.9372769727145744}]
["ANAMET-S",8130255,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 68",5,11.770821127265453,{"$f":"F898*(1-Elteq!$F$6)","v":11.770821127265453}]
["ANAMET-S",8130325,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight swivel with male thread, IP 68",5,19.583970746863123,{"$f":"F899*(1-Elteq!$F$6)","v":19.583970746863123}]
["ANAMET-S",8199124,"NPT 1/2\"","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 68",10,13.294431754630518,{"$f":"F900*(1-Elteq!$F$6)","v":13.294431754630518}]
["ANAMET-S",8199164,"NPT 1/2\"","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 68",10,17.317135423222421,{"$f":"F901*(1-Elteq!$F$6)","v":17.317135423222421}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8199204,"NPT 3/4\"","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 68",5,24.730801768571933,{"$f":"F902*(1-Elteq!$F$6)","v":24.730801768571933}]
["ANAMET-S",8199264,"NPT 1\"","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 68",5,39.418779828719273,{"$f":"F903*(1-Elteq!$F$6)","v":39.418779828719273}]
["ANAMET-S",7100115,"PG 11","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",10,3.4095432941644996,{"$f":"F904*(1-Elteq!$F$6)","v":3.4095432941644996}]
["ANAMET-S",7100135,"PG 13,5","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",10,3.4188336028679456,{"$f":"F905*(1-Elteq!$F$6)","v":3.4188336028679456}]
["ANAMET-S",7100165,"PG 16","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",10,4.0319939772953486,{"$f":"F906*(1-Elteq!$F$6)","v":4.0319939772953486}]
["ANAMET-S",7100215,"PG 21","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",5,6.1223134355705868,{"$f":"F907*(1-Elteq!$F$6)","v":6.1223134355705868}]
["ANAMET-S",7100295,"PG 29","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",5,9.9685012387970264,{"$f":"F908*(1-Elteq!$F$6)","v":9.9685012387970264}]
["ANAMET-S",7109115,"PG 11","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",10,6.2802486835291607,{"$f":"F909*(1-Elteq!$F$6)","v":6.2802486835291607}]
["ANAMET-S",7109135,"PG 13,5","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",10,6.4753451663015156,{"$f":"F910*(1-Elteq!$F$6)","v":6.4753451663015156}]
["ANAMET-S",7109165,"PG 16","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",10,7.6737949890459864,{"$f":"F911*(1-Elteq!$F$6)","v":7.6737949890459864}]
["ANAMET-S",7109215,"PG 21","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",5,11.24127353116906,{"$f":"F912*(1-Elteq!$F$6)","v":11.24127353116906}]
["ANAMET-S",7109295,"PG 29","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",5,20.996097669786842,{"$f":"F913*(1-Elteq!$F$6)","v":20.996097669786842}]
["ANAMET-S",8103115,"PG 11","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",10,5.759991396136213,{"$f":"F914*(1-Elteq!$F$6)","v":5.759991396136213}]
["ANAMET-S",8103135,"PG 13,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",10,5.759991396136213,{"$f":"F915*(1-Elteq!$F$6)","v":5.759991396136213}]
["ANAMET-S",8103165,"PG 16","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",10,6.1408940529774787,{"$f":"F916*(1-Elteq!$F$6)","v":6.1408940529774787}]
["ANAMET-S",8103215,"PG 21","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",5,9.0580509858593654,{"$f":"F917*(1-Elteq!$F$6)","v":9.0580509858593654}]
["ANAMET-S",8103295,"PG 29","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",5,12.969270950009925,{"$f":"F918*(1-Elteq!$F$6)","v":12.969270950009925}]
["ANAMET-S",8107115,"PG 11","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",10,12.161014092810165,{"$f":"F919*(1-Elteq!$F$6)","v":12.161014092810165}]
["ANAMET-S",8107155,"PG 13,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",10,13.907592129057921,{"$f":"F920*(1-Elteq!$F$6)","v":13.907592129057921}]
["ANAMET-S",8107165,"PG 16","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",10,16.954813383788046,{"$f":"F921*(1-Elteq!$F$6)","v":16.954813383788046}]
["ANAMET-S",8107215,"PG 21","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",5,25.631961712806145,{"$f":"F922*(1-Elteq!$F$6)","v":25.631961712806145}]
["ANAMET-S",8107295,"PG 29","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",5,36.780332156940752,{"$f":"F923*(1-Elteq!$F$6)","v":36.780332156940752}]
["ANAMET-S",8123165,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",10,5.4998627524397383,{"$f":"F924*(1-Elteq!$F$6)","v":5.4998627524397383}]
["ANAMET-S",8123205,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",10,5.90863633539134,{"$f":"F925*(1-Elteq!$F$6)","v":5.90863633539134}]
["ANAMET-S",8123255,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",5,8.7143095638318844,{"$f":"F926*(1-Elteq!$F$6)","v":8.7143095638318844}]
["ANAMET-S",8123325,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",5,12.476884588727312,{"$f":"F927*(1-Elteq!$F$6)","v":12.476884588727312}]
["ANAMET-S",8127165,"M16 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",10,12.030949770961927,{"$f":"F928*(1-Elteq!$F$6)","v":12.030949770961927}]
["ANAMET-S",8127175,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",10,12.161014092810165,{"$f":"F929*(1-Elteq!$F$6)","v":12.161014092810165}]
["ANAMET-S",8127205,"M20 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",10,13.898301820354476,{"$f":"F930*(1-Elteq!$F$6)","v":13.898301820354476}]
["ANAMET-S",8127225,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",10,16.954813383788046,{"$f":"F931*(1-Elteq!$F$6)","v":16.954813383788046}]
["ANAMET-S",8127255,"M25 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",5,23.170029906393086,{"$f":"F932*(1-Elteq!$F$6)","v":23.170029906393086}]
["ANAMET-S",8127285,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",5,25.631961712806145,{"$f":"F933*(1-Elteq!$F$6)","v":25.631961712806145}]
["ANAMET-S",8127325,"M32 x 1,5","Multiflex fittings for FCE / FCD, Straight cablehose male thread, IP 67",5,59.086363353913406,{"$f":"F934*(1-Elteq!$F$6)","v":59.086363353913406}]
["ANAMET-S",8139165,"M16 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 68",10,13.916882437761366,{"$f":"F935*(1-Elteq!$F$6)","v":13.916882437761366}]
["ANAMET-S",8139205,"M20 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 68",10,17.391457892849985,{"$f":"F936*(1-Elteq!$F$6)","v":17.391457892849985}]
["ANAMET-S",8139255,"M25 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 68",5,28.595570189205262,{"$f":"F937*(1-Elteq!$F$6)","v":28.595570189205262}]
["ANAMET-S",8139325,"M32 x 1,5","Multiflex fittings for FCE / FCD, 90° elbow swivel with male thread, IP 68",5,42.512452626966621,{"$f":"F938*(1-Elteq!$F$6)","v":42.512452626966621}]
["ANAMET-S",7140125,"NPT 1/2\"","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",10,4.1620582991435864,{"$f":"F939*(1-Elteq!$F$6)","v":4.1620582991435864}]
["ANAMET-S",7140165,"NPT 1/2\"","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",10,4.673025277833089,{"$f":"F940*(1-Elteq!$F$6)","v":4.673025277833089}]
["ANAMET-S",7140205,"NPT 3/4\"","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",5,6.4660548575980705,{"$f":"F941*(1-Elteq!$F$6)","v":6.4660548575980705}]
["ANAMET-S",7140265,"NPT 1\"","Multiflex fittings for FCE / FCD, Straight fixed with male thread, IP 68",5,11.324886309500069,{"$f":"F942*(1-Elteq!$F$6)","v":11.324886309500069}]
["ANAMET-S",7149125,"NPT 1/2\"","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",10,6.5682482533359723,{"$f":"F943*(1-Elteq!$F$6)","v":6.5682482533359723}]
["ANAMET-S",7149165,"NPT 1/2\"","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",10,7.8131496195976684,{"$f":"F944*(1-Elteq!$F$6)","v":7.8131496195976684}]
["ANAMET-S",7149205,"NPT 3/4\"","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",5,11.166951061541496,{"$f":"F945*(1-Elteq!$F$6)","v":11.166951061541496}]
["ANAMET-S",7149265,"NPT 1\"","Multiflex fittings for FCE / FCD, 90° elbow fixed with male thread, IP 68",5,20.698807791276582,{"$f":"F946*(1-Elteq!$F$6)","v":20.698807791276582}]
["ANAMET-S",7840125,"-","Multiflex fittings for FCE / FCD, Conduit connector, IP 68",10,6.1873455964947057,{"$f":"F947*(1-Elteq!$F$6)","v":6.1873455964947057}]
["ANAMET-S",7840165,"-","Multiflex fittings for FCE / FCD, Conduit connector, IP 68",10,7.5251500497908586,{"$f":"F948*(1-Elteq!$F$6)","v":7.5251500497908586}]
["ANAMET-S",7840205,"-","Multiflex fittings for FCE / FCD, Conduit connector, IP 68",5,11.315596000796624,{"$f":"F949*(1-Elteq!$F$6)","v":11.315596000796624}]
["ANAMET-S",7840265,"-","Multiflex fittings for FCE / FCD, Conduit connector, IP 68",5,20.299324517028428,{"$f":"F950*(1-Elteq!$F$6)","v":20.299324517028428}]
["ANAMET-S",8143125,"NPT 1/2\"","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",10,6.939860601473792,{"$f":"F951*(1-Elteq!$F$6)","v":6.939860601473792}]
["ANAMET-S",8143165,"NPT 1/2\"","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",10,7.4786985062736315,{"$f":"F952*(1-Elteq!$F$6)","v":7.4786985062736315}]
["ANAMET-S",8143205,"NPT 3/4\"","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",5,10.126436486755599,{"$f":"F953*(1-Elteq!$F$6)","v":10.126436486755599}]
["ANAMET-S",8143265,"NPT 1\"","Multiflex fittings for FCE / FCD, Straight fixed with female thread, IP 68",5,12.644110145389332,{"$f":"F954*(1-Elteq!$F$6)","v":12.644110145389332}]
["ANAMET-S",3100101,"5/16 \"","EF-M conduit with black cover, Galvanised steel core with PVC cover",30,4.8495411431985529,{"$f":"F955*(1-Elteq!$F$6)","v":4.8495411431985529}]
["ANAMET-S",3100121,"3/8\"","EF-M conduit with black cover, Galvanised steel core with PVC cover",75,4.1527679904401404,{"$f":"F956*(1-Elteq!$F$6)","v":4.1527679904401404}]
["ANAMET-S",3100125,"3/8\"","EF-M conduit with black cover, Galvanised steel core with PVC cover",240,4.1527679904401404,{"$f":"F957*(1-Elteq!$F$6)","v":4.1527679904401404}]
["ANAMET-S",3100161,"1/2\"","EF-M conduit with black cover, Galvanised steel core with PVC cover",60,4.8495411431985529,{"$f":"F958*(1-Elteq!$F$6)","v":4.8495411431985529}]
["ANAMET-S",3100165,"1/2\"","EF-M conduit with black cover, Galvanised steel core with PVC cover",150,4.8495411431985529,{"$f":"F959*(1-Elteq!$F$6)","v":4.8495411431985529}]
["ANAMET-S",3100201,"3/4\"","EF-M conduit with black cover, Galvanised steel core with PVC cover",30,6.4474742401911795,{"$f":"F960*(1-Elteq!$F$6)","v":6.4474742401911795}]
["ANAMET-S",3100205,"3/4\"","EF-M conduit with black cover, Galvanised steel core with PVC cover",150,6.4474742401911795,{"$f":"F961*(1-Elteq!$F$6)","v":6.4474742401911795}]
["ANAMET-S",3100261,"1\"","EF-M conduit with black cover, Galvanised steel core with PVC cover",30,9.5504373471419779,{"$f":"F962*(1-Elteq!$F$6)","v":9.5504373471419779}]
["ANAMET-S",3100265,"1\"","EF-M conduit with black cover, Galvanised steel core with PVC cover",120,9.5504373471419779,{"$f":"F963*(1-Elteq!$F$6)","v":9.5504373471419779}]
["ANAMET-S",3100351,"1 1/4\"","EF-M conduit with black cover, Galvanised steel core with PVC cover",15,13.935463055168256,{"$f":"F964*(1-Elteq!$F$6)","v":13.935463055168256}]
["ANAMET-S",3100355,"1 1/4\"","EF-M conduit with black cover, Galvanised steel core with PVC cover",75,13.935463055168256,{"$f":"F965*(1-Elteq!$F$6)","v":13.935463055168256}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},3100401,"1 1/2\"","EF-M conduit with black cover, Galvanised steel core with PVC cover",15,17.893134562836043,{"$f":"F966*(1-Elteq!$F$6)","v":17.893134562836043}]
["ANAMET-S",3100405,"1 1/2\"","EF-M conduit with black cover, Galvanised steel core with PVC cover",45,17.893134562836043,{"$f":"F967*(1-Elteq!$F$6)","v":17.893134562836043}]
["ANAMET-S",3100501,"2\"","EF-M conduit with black cover, Galvanised steel core with PVC cover",15,25.836348504281947,{"$f":"F968*(1-Elteq!$F$6)","v":25.836348504281947}]
["ANAMET-S",3100505,"2\"","EF-M conduit with black cover, Galvanised steel core with PVC cover",30,25.836348504281947,{"$f":"F969*(1-Elteq!$F$6)","v":25.836348504281947}]
["ANAMET-S",3140101,"5/16 \"","EF-M conduit with grey cover, Galvanised steel core with PVC cover",30,4.8495411431985529,{"$f":"F970*(1-Elteq!$F$6)","v":4.8495411431985529}]
["ANAMET-S",3140121,"3/8\"","EF-M conduit with grey cover, Galvanised steel core with PVC cover",75,4.1527679904401404,{"$f":"F971*(1-Elteq!$F$6)","v":4.1527679904401404}]
["ANAMET-S",3140125,"3/8\"","EF-M conduit with grey cover, Galvanised steel core with PVC cover",240,4.1527679904401404,{"$f":"F972*(1-Elteq!$F$6)","v":4.1527679904401404}]
["ANAMET-S",3140161,"1/2\"","EF-M conduit with grey cover, Galvanised steel core with PVC cover",60,4.8495411431985529,{"$f":"F973*(1-Elteq!$F$6)","v":4.8495411431985529}]
["ANAMET-S",3140165,"1/2\"","EF-M conduit with grey cover, Galvanised steel core with PVC cover",150,4.8495411431985529,{"$f":"F974*(1-Elteq!$F$6)","v":4.8495411431985529}]
["ANAMET-S",3140201,"3/4\"","EF-M conduit with grey cover, Galvanised steel core with PVC cover",30,6.4474742401911795,{"$f":"F975*(1-Elteq!$F$6)","v":6.4474742401911795}]
["ANAMET-S",3140205,"3/4\"","EF-M conduit with grey cover, Galvanised steel core with PVC cover",150,6.4474742401911795,{"$f":"F976*(1-Elteq!$F$6)","v":6.4474742401911795}]
["ANAMET-S",3140261,"1\"","EF-M conduit with grey cover, Galvanised steel core with PVC cover",30,9.5504373471419779,{"$f":"F977*(1-Elteq!$F$6)","v":9.5504373471419779}]
["ANAMET-S",3140265,"1\"","EF-M conduit with grey cover, Galvanised steel core with PVC cover",120,9.5504373471419779,{"$f":"F978*(1-Elteq!$F$6)","v":9.5504373471419779}]
["ANAMET-S",3140351,"1 1/4\"","EF-M conduit with grey cover, Galvanised steel core with PVC cover",15,13.935463055168256,{"$f":"F979*(1-Elteq!$F$6)","v":13.935463055168256}]
["ANAMET-S",3140355,"1 1/4\"","EF-M conduit with grey cover, Galvanised steel core with PVC cover",75,13.935463055168256,{"$f":"F980*(1-Elteq!$F$6)","v":13.935463055168256}]
["ANAMET-S",3140401,"1 1/2\"","EF-M conduit with grey cover, Galvanised steel core with PVC cover",15,17.893134562836043,{"$f":"F981*(1-Elteq!$F$6)","v":17.893134562836043}]
["ANAMET-S",3140405,"1 1/2\"","EF-M conduit with grey cover, Galvanised steel core with PVC cover",45,17.893134562836043,{"$f":"F982*(1-Elteq!$F$6)","v":17.893134562836043}]
["ANAMET-S",3140501,"2\"","EF-M conduit with grey cover, Galvanised steel core with PVC cover",15,25.836348504281947,{"$f":"F983*(1-Elteq!$F$6)","v":25.836348504281947}]
["ANAMET-S",3140505,"2\"","EF-M conduit with grey cover, Galvanised steel core with PVC cover",30,25.836348504281947,{"$f":"F984*(1-Elteq!$F$6)","v":25.836348504281947}]
["ANAMET-S",3110061,"1/4\"","EF conduit with grey cover, Galvanised steel core with PVC cover",50,8.0918588807010359,{"$f":"F985*(1-Elteq!$F$6)","v":8.0918588807010359}]
["ANAMET-S",3110101,"5/16 \"","EF conduit with grey cover, Galvanised steel core with PVC cover",50,6.0758618920533598,{"$f":"F986*(1-Elteq!$F$6)","v":6.0758618920533598}]
["ANAMET-S",3110103,"5/16 \"","EF conduit with grey cover, Galvanised steel core with PVC cover",10,6.0758618920533598,{"$f":"F987*(1-Elteq!$F$6)","v":6.0758618920533598}]
["ANAMET-S",3110121,"3/8\"","EF conduit with grey cover, Galvanised steel core with PVC cover",75,5.1839922565225915,{"$f":"F988*(1-Elteq!$F$6)","v":5.1839922565225915}]
["ANAMET-S",3110123,"3/8\"","EF conduit with grey cover, Galvanised steel core with PVC cover",10,5.1839922565225915,{"$f":"F989*(1-Elteq!$F$6)","v":5.1839922565225915}]
["ANAMET-S",3110125,"3/8\"","EF conduit with grey cover, Galvanised steel core with PVC cover",250,5.1839922565225915,{"$f":"F990*(1-Elteq!$F$6)","v":5.1839922565225915}]
["ANAMET-S",3110161,"1/2\"","EF conduit with grey cover, Galvanised steel core with PVC cover",60,6.0758618920533598,{"$f":"F991*(1-Elteq!$F$6)","v":6.0758618920533598}]
["ANAMET-S",3110163,"1/2\"","EF conduit with grey cover, Galvanised steel core with PVC cover",10,6.0758618920533598,{"$f":"F992*(1-Elteq!$F$6)","v":6.0758618920533598}]
["ANAMET-S",3110165,"1/2\"","EF conduit with grey cover, Galvanised steel core with PVC cover",150,6.0758618920533598,{"$f":"F993*(1-Elteq!$F$6)","v":6.0758618920533598}]
["ANAMET-S",3110201,"3/4\"","EF conduit with grey cover, Galvanised steel core with PVC cover",50,8.0732782632941422,{"$f":"F994*(1-Elteq!$F$6)","v":8.0732782632941422}]
["ANAMET-S",3110203,"3/4\"","EF conduit with grey cover, Galvanised steel core with PVC cover",10,8.0732782632941422,{"$f":"F995*(1-Elteq!$F$6)","v":8.0732782632941422}]
["ANAMET-S",3110205,"3/4\"","EF conduit with grey cover, Galvanised steel core with PVC cover",120,8.0732782632941422,{"$f":"F996*(1-Elteq!$F$6)","v":8.0732782632941422}]
["ANAMET-S",3110261,"1\"","EF conduit with grey cover, Galvanised steel core with PVC cover",30,13.65675379406489,{"$f":"F997*(1-Elteq!$F$6)","v":13.65675379406489}]
["ANAMET-S",3110263,"1\"","EF conduit with grey cover, Galvanised steel core with PVC cover",10,13.65675379406489,{"$f":"F998*(1-Elteq!$F$6)","v":13.65675379406489}]
["ANAMET-S",3110265,"1\"","EF conduit with grey cover, Galvanised steel core with PVC cover",90,13.65675379406489,{"$f":"F999*(1-Elteq!$F$6)","v":13.65675379406489}]
["ANAMET-S",3110351,"1 1/4\"","EF conduit with grey cover, Galvanised steel core with PVC cover",30,17.744489623580915,{"$f":"F1000*(1-Elteq!$F$6)","v":17.744489623580915}]
["ANAMET-S",3110353,"1 1/4\"","EF conduit with grey cover, Galvanised steel core with PVC cover",10,17.744489623580915,{"$f":"F1001*(1-Elteq!$F$6)","v":17.744489623580915}]
["ANAMET-S",3110355,"1 1/4\"","EF conduit with grey cover, Galvanised steel core with PVC cover",60,17.744489623580915,{"$f":"F1002*(1-Elteq!$F$6)","v":17.744489623580915}]
["ANAMET-S",3110401,"1 1/2\"","EF conduit with grey cover, Galvanised steel core with PVC cover",15,34.699303007368961,{"$f":"F1003*(1-Elteq!$F$6)","v":34.699303007368961}]
["ANAMET-S",3110405,"1 1/2\"","EF conduit with grey cover, Galvanised steel core with PVC cover",45,34.699303007368961,{"$f":"F1004*(1-Elteq!$F$6)","v":34.699303007368961}]
["ANAMET-S",3110501,"2\"","EF conduit with grey cover, Galvanised steel core with PVC cover",15,39.335167050388264,{"$f":"F1005*(1-Elteq!$F$6)","v":39.335167050388264}]
["ANAMET-S",3110505,"2\"","EF conduit with grey cover, Galvanised steel core with PVC cover",30,39.335167050388264,{"$f":"F1006*(1-Elteq!$F$6)","v":39.335167050388264}]
["ANAMET-S",3110631,"2 1/2\"","EF conduit with grey cover, Galvanised steel core with PVC cover",7.5,83.371230304719944,{"$f":"F1007*(1-Elteq!$F$6)","v":83.371230304719944}]
["ANAMET-S",3110751,"3\"","EF conduit with grey cover, Galvanised steel core with PVC cover",7.5,117.77324343357866,{"$f":"F1008*(1-Elteq!$F$6)","v":117.77324343357866}]
["ANAMET-S",3111001,"4\"","EF conduit with grey cover, Galvanised steel core with PVC cover",7.5,181.39327743477347,{"$f":"F1009*(1-Elteq!$F$6)","v":181.39327743477347}]
["ANAMET-S",3111251,"5\"","EF conduit with grey cover, Galvanised steel core with PVC cover",7.5,249.89072350527718,{"$f":"F1010*(1-Elteq!$F$6)","v":249.89072350527718}]
["ANAMET-S",3111501,"6\"","EF conduit with grey cover, Galvanised steel core with PVC cover",7.5,328.31950957976409,{"$f":"F1011*(1-Elteq!$F$6)","v":328.31950957976409}]
["ANAMET-S",3150061,"1/4\"","EF conduit with black cover, Galvanised steel core with PVC cover",50,8.0918588807010359,{"$f":"F1012*(1-Elteq!$F$6)","v":8.0918588807010359}]
["ANAMET-S",3150101,"5/16 \"","EF conduit with black cover, Galvanised steel core with PVC cover",50,6.0758618920533598,{"$f":"F1013*(1-Elteq!$F$6)","v":6.0758618920533598}]
["ANAMET-S",3150103,"5/16 \"","EF conduit with black cover, Galvanised steel core with PVC cover",10,6.0758618920533598,{"$f":"F1014*(1-Elteq!$F$6)","v":6.0758618920533598}]
["ANAMET-S",3150121,"3/8\"","EF conduit with black cover, Galvanised steel core with PVC cover",75,5.1839922565225915,{"$f":"F1015*(1-Elteq!$F$6)","v":5.1839922565225915}]
["ANAMET-S",3150123,"3/8\"","EF conduit with black cover, Galvanised steel core with PVC cover",10,5.1839922565225915,{"$f":"F1016*(1-Elteq!$F$6)","v":5.1839922565225915}]
["ANAMET-S",3150125,"3/8\"","EF conduit with black cover, Galvanised steel core with PVC cover",250,5.1839922565225915,{"$f":"F1017*(1-Elteq!$F$6)","v":5.1839922565225915}]
["ANAMET-S",3150161,"1/2\"","EF conduit with black cover, Galvanised steel core with PVC cover",60,6.0758618920533598,{"$f":"F1018*(1-Elteq!$F$6)","v":6.0758618920533598}]
["ANAMET-S",3150163,"1/2\"","EF conduit with black cover, Galvanised steel core with PVC cover",10,6.0758618920533598,{"$f":"F1019*(1-Elteq!$F$6)","v":6.0758618920533598}]
["ANAMET-S",3150165,"1/2\"","EF conduit with black cover, Galvanised steel core with PVC cover",150,6.0758618920533598,{"$f":"F1020*(1-Elteq!$F$6)","v":6.0758618920533598}]
["ANAMET-S",3150201,"3/4\"","EF conduit with black cover, Galvanised steel core with PVC cover",50,8.0732782632941422,{"$f":"F1021*(1-Elteq!$F$6)","v":8.0732782632941422}]
["ANAMET-S",3150203,"3/4\"","EF conduit with black cover, Galvanised steel core with PVC cover",10,8.0732782632941422,{"$f":"F1022*(1-Elteq!$F$6)","v":8.0732782632941422}]
["ANAMET-S",3150205,"3/4\"","EF conduit with black cover, Galvanised steel core with PVC cover",120,8.0732782632941422,{"$f":"F1023*(1-Elteq!$F$6)","v":8.0732782632941422}]
["ANAMET-S",3150261,"1\"","EF conduit with black cover, Galvanised steel core with PVC cover",30,13.65675379406489,{"$f":"F1024*(1-Elteq!$F$6)","v":13.65675379406489}]
["ANAMET-S",3150263,"1\"","EF conduit with black cover, Galvanised steel core with PVC cover",10,13.65675379406489,{"$f":"F1025*(1-Elteq!$F$6)","v":13.65675379406489}]
["ANAMET-S",3150265,"1\"","EF conduit with black cover, Galvanised steel core with PVC cover",90,13.65675379406489,{"$f":"F1026*(1-Elteq!$F$6)","v":13.65675379406489}]
["ANAMET-S",3150351,"1 1/4\"","EF conduit with black cover, Galvanised steel core with PVC cover",30,17.744489623580915,{"$f":"F1027*(1-Elteq!$F$6)","v":17.744489623580915}]
["ANAMET-S",3150353,"1 1/4\"","EF conduit with black cover, Galvanised steel core with PVC cover",10,17.744489623580915,{"$f":"F1028*(1-Elteq!$F$6)","v":17.744489623580915}]
["ANAMET-S",3150355,"1 1/4\"","EF conduit with black cover, Galvanised steel core with PVC cover",60,17.744489623580915,{"$f":"F1029*(1-Elteq!$F$6)","v":17.744489623580915}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},3150401,"1 1/2\"","EF conduit with black cover, Galvanised steel core with PVC cover",15,34.699303007368961,{"$f":"F1030*(1-Elteq!$F$6)","v":34.699303007368961}]
["ANAMET-S",3150405,"1 1/2\"","EF conduit with black cover, Galvanised steel core with PVC cover",45,34.699303007368961,{"$f":"F1031*(1-Elteq!$F$6)","v":34.699303007368961}]
["ANAMET-S",3150501,"2\"","EF conduit with black cover, Galvanised steel core with PVC cover",15,39.335167050388264,{"$f":"F1032*(1-Elteq!$F$6)","v":39.335167050388264}]
["ANAMET-S",3150505,"2\"","EF conduit with black cover, Galvanised steel core with PVC cover",30,39.335167050388264,{"$f":"F1033*(1-Elteq!$F$6)","v":39.335167050388264}]
["ANAMET-S",3150631,"2 1/2\"","EF conduit with black cover, Galvanised steel core with PVC cover",7.5,83.371230304719944,{"$f":"F1034*(1-Elteq!$F$6)","v":83.371230304719944}]
["ANAMET-S",3150751,"3\"","EF conduit with black cover, Galvanised steel core with PVC cover",7.5,117.77324343357866,{"$f":"F1035*(1-Elteq!$F$6)","v":117.77324343357866}]
["ANAMET-S",3151001,"4\"","EF conduit with black cover, Galvanised steel core with PVC cover",7.5,181.39327743477347,{"$f":"F1036*(1-Elteq!$F$6)","v":181.39327743477347}]
["ANAMET-S",3151251,"5\"","EF conduit with black cover, Galvanised steel core with PVC cover",7.5,249.89072350527718,{"$f":"F1037*(1-Elteq!$F$6)","v":249.89072350527718}]
["ANAMET-S",3151501,"6\"","EF conduit with black cover, Galvanised steel core with PVC cover",7.5,328.31950957976409,{"$f":"F1038*(1-Elteq!$F$6)","v":328.31950957976409}]
["ANAMET-S",3200061,"1/4\"","OR conduit with black cover, Galvanised steel core with PVC cover",50,10.005662473610808,{"$f":"F1039*(1-Elteq!$F$6)","v":10.005662473610808}]
["ANAMET-S",3200101,"5/16 \"","OR conduit with black cover, Galvanised steel core with PVC cover",50,7.3857954192391757,{"$f":"F1040*(1-Elteq!$F$6)","v":7.3857954192391757}]
["ANAMET-S",3200103,"5/16 \"","OR conduit with black cover, Galvanised steel core with PVC cover",10,7.3857954192391757,{"$f":"F1041*(1-Elteq!$F$6)","v":7.3857954192391757}]
["ANAMET-S",3200121,"3/8\"","OR conduit with black cover, Galvanised steel core with PVC cover",75,6.2245068313084877,{"$f":"F1042*(1-Elteq!$F$6)","v":6.2245068313084877}]
["ANAMET-S",3200123,"3/8\"","OR conduit with black cover, Galvanised steel core with PVC cover",10,6.2245068313084877,{"$f":"F1043*(1-Elteq!$F$6)","v":6.2245068313084877}]
["ANAMET-S",3200125,"3/8\"","OR conduit with black cover, Galvanised steel core with PVC cover",250,6.2245068313084877,{"$f":"F1044*(1-Elteq!$F$6)","v":6.2245068313084877}]
["ANAMET-S",3200161,"1/2\"","OR conduit with black cover, Galvanised steel core with PVC cover",60,7.2650214060943847,{"$f":"F1045*(1-Elteq!$F$6)","v":7.2650214060943847}]
["ANAMET-S",3200163,"1/2\"","OR conduit with black cover, Galvanised steel core with PVC cover",10,7.2650214060943847,{"$f":"F1046*(1-Elteq!$F$6)","v":7.2650214060943847}]
["ANAMET-S",3200165,"1/2\"","OR conduit with black cover, Galvanised steel core with PVC cover",150,7.2650214060943847,{"$f":"F1047*(1-Elteq!$F$6)","v":7.2650214060943847}]
["ANAMET-S",3200201,"3/4\"","OR conduit with black cover, Galvanised steel core with PVC cover",50,9.6805016689902157,{"$f":"F1048*(1-Elteq!$F$6)","v":9.6805016689902157}]
["ANAMET-S",3200203,"3/4\"","OR conduit with black cover, Galvanised steel core with PVC cover",10,9.6805016689902157,{"$f":"F1049*(1-Elteq!$F$6)","v":9.6805016689902157}]
["ANAMET-S",3200205,"3/4\"","OR conduit with black cover, Galvanised steel core with PVC cover",120,9.6805016689902157,{"$f":"F1050*(1-Elteq!$F$6)","v":9.6805016689902157}]
["ANAMET-S",3200261,"1\"","OR conduit with black cover, Galvanised steel core with PVC cover",30,16.38810455287787,{"$f":"F1051*(1-Elteq!$F$6)","v":16.38810455287787}]
["ANAMET-S",3200263,"1\"","OR conduit with black cover, Galvanised steel core with PVC cover",10,16.38810455287787,{"$f":"F1052*(1-Elteq!$F$6)","v":16.38810455287787}]
["ANAMET-S",3200265,"1\"","OR conduit with black cover, Galvanised steel core with PVC cover",90,16.38810455287787,{"$f":"F1053*(1-Elteq!$F$6)","v":16.38810455287787}]
["ANAMET-S",3200351,"1 1/4\"","OR conduit with black cover, Galvanised steel core with PVC cover",30,21.293387548297098,{"$f":"F1054*(1-Elteq!$F$6)","v":21.293387548297098}]
["ANAMET-S",3200353,"1 1/4\"","OR conduit with black cover, Galvanised steel core with PVC cover",10,21.293387548297098,{"$f":"F1055*(1-Elteq!$F$6)","v":21.293387548297098}]
["ANAMET-S",3200355,"1 1/4\"","OR conduit with black cover, Galvanised steel core with PVC cover",60,21.293387548297098,{"$f":"F1056*(1-Elteq!$F$6)","v":21.293387548297098}]
["ANAMET-S",3200401,"1 1/2\"","OR conduit with black cover, Galvanised steel core with PVC cover",15,41.648453917546199,{"$f":"F1057*(1-Elteq!$F$6)","v":41.648453917546199}]
["ANAMET-S",3200405,"1 1/2\"","OR conduit with black cover, Galvanised steel core with PVC cover",45,41.648453917546199,{"$f":"F1058*(1-Elteq!$F$6)","v":41.648453917546199}]
["ANAMET-S",3200501,"2\"","OR conduit with black cover, Galvanised steel core with PVC cover",15,56.540818769169334,{"$f":"F1059*(1-Elteq!$F$6)","v":56.540818769169334}]
["ANAMET-S",3200505,"2\"","OR conduit with black cover, Galvanised steel core with PVC cover",30,56.540818769169334,{"$f":"F1060*(1-Elteq!$F$6)","v":56.540818769169334}]
["ANAMET-S",3200631,"2 1/2\"","OR conduit with black cover, Galvanised steel core with PVC cover",15,97.213790272853757,{"$f":"F1061*(1-Elteq!$F$6)","v":97.213790272853757}]
["ANAMET-S",3200751,"3\"","OR conduit with black cover, Galvanised steel core with PVC cover",7.5,141.31488568810957,{"$f":"F1062*(1-Elteq!$F$6)","v":141.31488568810957}]
["ANAMET-S",3201001,"4\"","OR conduit with black cover, Galvanised steel core with PVC cover",7.5,217.68122323043161,{"$f":"F1063*(1-Elteq!$F$6)","v":217.68122323043161}]
["ANAMET-S",3220121,"3/8\"","OR conduit with blue cover, Galvanised steel core with PVC cover",30,6.6611513403704263,{"$f":"F1064*(1-Elteq!$F$6)","v":6.6611513403704263}]
["ANAMET-S",3220161,"1/2\"","OR conduit with blue cover, Galvanised steel core with PVC cover",30,7.6273434455287594,{"$f":"F1065*(1-Elteq!$F$6)","v":7.6273434455287594}]
["ANAMET-S",3220201,"3/4\"","OR conduit with blue cover, Galvanised steel core with PVC cover",30,10.163597721569381,{"$f":"F1066*(1-Elteq!$F$6)","v":10.163597721569381}]
["ANAMET-S",3220261,"1\"","OR conduit with blue cover, Galvanised steel core with PVC cover",30,17.205651718781073,{"$f":"F1067*(1-Elteq!$F$6)","v":17.205651718781073}]
["ANAMET-S",3220351,"1 1/4\"","OR conduit with blue cover, Galvanised steel core with PVC cover",30,22.352482740489879,{"$f":"F1068*(1-Elteq!$F$6)","v":22.352482740489879}]
["ANAMET-S",3170061,"1/4\"","HC conduit with black cover, Galvanised steel core with PVC cover",50,11.25985414857595,{"$f":"F1069*(1-Elteq!$F$6)","v":11.25985414857595}]
["ANAMET-S",3170101,"5/16 \"","HC conduit with black cover, Galvanised steel core with PVC cover",50,8.4263099940250736,{"$f":"F1070*(1-Elteq!$F$6)","v":8.4263099940250736}]
["ANAMET-S",3170103,"5/16 \"","HC conduit with black cover, Galvanised steel core with PVC cover",10,8.4263099940250736,{"$f":"F1071*(1-Elteq!$F$6)","v":8.4263099940250736}]
["ANAMET-S",3170121,"3/8\"","HC conduit with black cover, Galvanised steel core with PVC cover",75,7.1721183190599289,{"$f":"F1072*(1-Elteq!$F$6)","v":7.1721183190599289}]
["ANAMET-S",3170123,"3/8\"","HC conduit with black cover, Galvanised steel core with PVC cover",10,7.1721183190599289,{"$f":"F1073*(1-Elteq!$F$6)","v":7.1721183190599289}]
["ANAMET-S",3170125,"3/8\"","HC conduit with black cover, Galvanised steel core with PVC cover",250,7.1721183190599289,{"$f":"F1074*(1-Elteq!$F$6)","v":7.1721183190599289}]
["ANAMET-S",3170161,"1/2\"","HC conduit with black cover, Galvanised steel core with PVC cover",60,8.3612778331009547,{"$f":"F1075*(1-Elteq!$F$6)","v":8.3612778331009547}]
["ANAMET-S",3170163,"1/2\"","HC conduit with black cover, Galvanised steel core with PVC cover",10,8.3612778331009547,{"$f":"F1076*(1-Elteq!$F$6)","v":8.3612778331009547}]
["ANAMET-S",3170165,"1/2\"","HC conduit with black cover, Galvanised steel core with PVC cover",150,8.3612778331009547,{"$f":"F1077*(1-Elteq!$F$6)","v":8.3612778331009547}]
["ANAMET-S",3170201,"3/4\"","HC conduit with black cover, Galvanised steel core with PVC cover",50,11.111209209320824,{"$f":"F1078*(1-Elteq!$F$6)","v":11.111209209320824}]
["ANAMET-S",3170203,"3/4\"","HC conduit with black cover, Galvanised steel core with PVC cover",10,11.111209209320824,{"$f":"F1079*(1-Elteq!$F$6)","v":11.111209209320824}]
["ANAMET-S",3170205,"3/4\"","HC conduit with black cover, Galvanised steel core with PVC cover",120,11.111209209320824,{"$f":"F1080*(1-Elteq!$F$6)","v":11.111209209320824}]
["ANAMET-S",3170261,"1\"","HC conduit with black cover, Galvanised steel core with PVC cover",30,18.840746050587484,{"$f":"F1081*(1-Elteq!$F$6)","v":18.840746050587484}]
["ANAMET-S",3170263,"1\"","HC conduit with black cover, Galvanised steel core with PVC cover",10,18.840746050587484,{"$f":"F1082*(1-Elteq!$F$6)","v":18.840746050587484}]
["ANAMET-S",3170265,"1\"","HC conduit with black cover, Galvanised steel core with PVC cover",90,18.840746050587484,{"$f":"F1083*(1-Elteq!$F$6)","v":18.840746050587484}]
["ANAMET-S",3170351,"1 1/4\"","HC conduit with black cover, Galvanised steel core with PVC cover",30,24.498544050985796,{"$f":"F1084*(1-Elteq!$F$6)","v":24.498544050985796}]
["ANAMET-S",3170353,"1 1/4\"","HC conduit with black cover, Galvanised steel core with PVC cover",10,24.498544050985796,{"$f":"F1085*(1-Elteq!$F$6)","v":24.498544050985796}]
["ANAMET-S",3170355,"1 1/4\"","HC conduit with black cover, Galvanised steel core with PVC cover",60,24.498544050985796,{"$f":"F1086*(1-Elteq!$F$6)","v":24.498544050985796}]
["ANAMET-S",3170401,"1 1/2\"","HC conduit with black cover, Galvanised steel core with PVC cover",15,47.872960748854688,{"$f":"F1087*(1-Elteq!$F$6)","v":47.872960748854688}]
["ANAMET-S",3170405,"1 1/2\"","HC conduit with black cover, Galvanised steel core with PVC cover",45,47.872960748854688,{"$f":"F1088*(1-Elteq!$F$6)","v":47.872960748854688}]
["ANAMET-S",3170501,"2\"","HC conduit with black cover, Galvanised steel core with PVC cover",15,54.246112519418304,{"$f":"F1089*(1-Elteq!$F$6)","v":54.246112519418304}]
["ANAMET-S",3170505,"2\"","HC conduit with black cover, Galvanised steel core with PVC cover",30,54.246112519418304,{"$f":"F1090*(1-Elteq!$F$6)","v":54.246112519418304}]
["ANAMET-S",3260121,"3/8\"","HCX conduit with black cover, Galvanised steel core with TPE cover",30,10.06140432583148,{"$f":"F1091*(1-Elteq!$F$6)","v":10.06140432583148}]
["ANAMET-S",3260123,"3/8\"","HCX conduit with black cover, Galvanised steel core with TPE cover",10,10.06140432583148,{"$f":"F1092*(1-Elteq!$F$6)","v":10.06140432583148}]
["ANAMET-S",3260125,"3/8\"","HCX conduit with black cover, Galvanised steel core with TPE cover",250,10.06140432583148,{"$f":"F1093*(1-Elteq!$F$6)","v":10.06140432583148}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},3260161,"1/2\"","HCX conduit with black cover, Galvanised steel core with TPE cover",30,11.742950201155118,{"$f":"F1094*(1-Elteq!$F$6)","v":11.742950201155118}]
["ANAMET-S",3260163,"1/2\"","HCX conduit with black cover, Galvanised steel core with TPE cover",10,11.742950201155118,{"$f":"F1095*(1-Elteq!$F$6)","v":11.742950201155118}]
["ANAMET-S",3260165,"1/2\"","HCX conduit with black cover, Galvanised steel core with TPE cover",150,11.742950201155118,{"$f":"F1096*(1-Elteq!$F$6)","v":11.742950201155118}]
["ANAMET-S",3260201,"3/4\"","HCX conduit with black cover, Galvanised steel core with TPE cover",30,15.617008930491892,{"$f":"F1097*(1-Elteq!$F$6)","v":15.617008930491892}]
["ANAMET-S",3260203,"3/4\"","HCX conduit with black cover, Galvanised steel core with TPE cover",10,15.617008930491892,{"$f":"F1098*(1-Elteq!$F$6)","v":15.617008930491892}]
["ANAMET-S",3260205,"3/4\"","HCX conduit with black cover, Galvanised steel core with TPE cover",120,15.617008930491892,{"$f":"F1099*(1-Elteq!$F$6)","v":15.617008930491892}]
["ANAMET-S",3260261,"1\"","HCX conduit with black cover, Galvanised steel core with TPE cover",30,26.468089496116239,{"$f":"F1100*(1-Elteq!$F$6)","v":26.468089496116239}]
["ANAMET-S",3260263,"1\"","HCX conduit with black cover, Galvanised steel core with TPE cover",10,26.468089496116239,{"$f":"F1101*(1-Elteq!$F$6)","v":26.468089496116239}]
["ANAMET-S",3260265,"1\"","HCX conduit with black cover, Galvanised steel core with TPE cover",90,26.468089496116239,{"$f":"F1102*(1-Elteq!$F$6)","v":26.468089496116239}]
["ANAMET-S",3260351,"1 1/4\"","HCX conduit with black cover, Galvanised steel core with TPE cover",15,34.374142202748359,{"$f":"F1103*(1-Elteq!$F$6)","v":34.374142202748359}]
["ANAMET-S",3260355,"1 1/4\"","HCX conduit with black cover, Galvanised steel core with TPE cover",60,34.374142202748359,{"$f":"F1104*(1-Elteq!$F$6)","v":34.374142202748359}]
["ANAMET-S",3260401,"1 1/2\"","HCX conduit with black cover, Galvanised steel core with TPE cover",15,67.196802852021321,{"$f":"F1105*(1-Elteq!$F$6)","v":67.196802852021321}]
["ANAMET-S",3260405,"1 1/2\"","HCX conduit with black cover, Galvanised steel core with TPE cover",45,67.196802852021321,{"$f":"F1106*(1-Elteq!$F$6)","v":67.196802852021321}]
["ANAMET-S",3260501,"2\"","HCX conduit with black cover, Galvanised steel core with TPE cover",15,76.134079824735906,{"$f":"F1107*(1-Elteq!$F$6)","v":76.134079824735906}]
["ANAMET-S",3260505,"2\"","HCX conduit with black cover, Galvanised steel core with TPE cover",30,76.134079824735906,{"$f":"F1108*(1-Elteq!$F$6)","v":76.134079824735906}]
["ANAMET-S",3310061,"1/4\"","HFX conduit with black cover, Galvanised steel core with TPU cover",30,14.037656450906157,{"$f":"F1109*(1-Elteq!$F$6)","v":14.037656450906157}]
["ANAMET-S",3310101,"5/16 \"","HFX conduit with black cover, Galvanised steel core with TPU cover",30,10.544500378410646,{"$f":"F1110*(1-Elteq!$F$6)","v":10.544500378410646}]
["ANAMET-S",3310103,"5/16\"","HFX conduit with black cover, Galvanised steel core with TPU cover",10,10.544500378410646,{"$f":"F1111*(1-Elteq!$F$6)","v":10.544500378410646}]
["ANAMET-S",3310121,"3/8\"","HFX conduit with black cover, Galvanised steel core with TPU cover",30,9.1323734554869311,{"$f":"F1112*(1-Elteq!$F$6)","v":9.1323734554869311}]
["ANAMET-S",3310123,"3/8\"","HFX conduit with black cover, Galvanised steel core with TPU cover",10,9.1323734554869311,{"$f":"F1113*(1-Elteq!$F$6)","v":9.1323734554869311}]
["ANAMET-S",3310125,"3/8\"","HFX conduit with black cover, Galvanised steel core with TPU cover",250,9.1323734554869311,{"$f":"F1114*(1-Elteq!$F$6)","v":9.1323734554869311}]
["ANAMET-S",3310161,"1/2\"","HFX conduit with black cover, Galvanised steel core with TPU cover",30,11.585014953196543,{"$f":"F1115*(1-Elteq!$F$6)","v":11.585014953196543}]
["ANAMET-S",3310163,"1/2\"","HFX conduit with black cover, Galvanised steel core with TPU cover",10,11.585014953196543,{"$f":"F1116*(1-Elteq!$F$6)","v":11.585014953196543}]
["ANAMET-S",3310165,"1/2\"","HFX conduit with black cover, Galvanised steel core with TPU cover",150,11.585014953196543,{"$f":"F1117*(1-Elteq!$F$6)","v":11.585014953196543}]
["ANAMET-S",3310201,"3/4\"","HFX conduit with black cover, Galvanised steel core with TPU cover",30,12.876367862975467,{"$f":"F1118*(1-Elteq!$F$6)","v":12.876367862975467}]
["ANAMET-S",3310203,"3/4\"","HFX conduit with black cover, Galvanised steel core with TPU cover",10,12.876367862975467,{"$f":"F1119*(1-Elteq!$F$6)","v":12.876367862975467}]
["ANAMET-S",3310205,"3/4\"","HFX conduit with black cover, Galvanised steel core with TPU cover",120,12.876367862975467,{"$f":"F1120*(1-Elteq!$F$6)","v":12.876367862975467}]
["ANAMET-S",3310261,"1\"","HFX conduit with black cover, Galvanised steel core with TPU cover",30,18.366940306711761,{"$f":"F1121*(1-Elteq!$F$6)","v":18.366940306711761}]
["ANAMET-S",3310263,"1\"","HFX conduit with black cover, Galvanised steel core with TPU cover",10,18.366940306711761,{"$f":"F1122*(1-Elteq!$F$6)","v":18.366940306711761}]
["ANAMET-S",3310265,"1\"","HFX conduit with black cover, Galvanised steel core with TPU cover",90,18.366940306711761,{"$f":"F1123*(1-Elteq!$F$6)","v":18.366940306711761}]
["ANAMET-S",3310351,"1 1/4\"","HFX conduit with black cover, Galvanised steel core with TPU cover",15,22.473256753634676,{"$f":"F1124*(1-Elteq!$F$6)","v":22.473256753634676}]
["ANAMET-S",3310355,"1 1/4\"","HFX conduit with black cover, Galvanised steel core with TPU cover",60,22.473256753634676,{"$f":"F1125*(1-Elteq!$F$6)","v":22.473256753634676}]
["ANAMET-S",3310401,"1 1/2\"","HFX conduit with black cover, Galvanised steel core with TPU cover",15,72.102085847440563,{"$f":"F1126*(1-Elteq!$F$6)","v":72.102085847440563}]
["ANAMET-S",3310501,"2\"","HFX conduit with black cover, Galvanised steel core with TPU cover",15,81.680394120692867,{"$f":"F1127*(1-Elteq!$F$6)","v":81.680394120692867}]
["ANAMET-S",3352121,"3/8\"","HFX conduit with blue cover, Galvanised steel core with TPU cover",30,9.8570175343556787,{"$f":"F1128*(1-Elteq!$F$6)","v":9.8570175343556787}]
["ANAMET-S",3352161,"1/2\"","HFX conduit with blue cover, Galvanised steel core with TPU cover",30,12.523336132244539,{"$f":"F1129*(1-Elteq!$F$6)","v":12.523336132244539}]
["ANAMET-S",3352201,"3/4\"","HFX conduit with blue cover, Galvanised steel core with TPU cover",30,13.916882437761366,{"$f":"F1130*(1-Elteq!$F$6)","v":13.916882437761366}]
["ANAMET-S",3352261,"1 \"","HFX conduit with blue cover, Galvanised steel core with TPU cover",30,19.853389699263044,{"$f":"F1131*(1-Elteq!$F$6)","v":19.853389699263044}]
["ANAMET-S",3352351,"1 1/4\"","HFX conduit with blue cover, Galvanised steel core with TPU cover",15,24.275576642103101,{"$f":"F1132*(1-Elteq!$F$6)","v":24.275576642103101}]
["ANAMET-S",3352401,"1.1/2","HFX conduit with blue cover, Galvanised steel core with TPU cover",15,75.706725624377398,{"$f":"F1133*(1-Elteq!$F$6)","v":75.706725624377398}]
["ANAMET-S",3352501,2,"HFX conduit with blue cover, Galvanised steel core with TPU cover",15,85.758839641505446,{"$f":"F1134*(1-Elteq!$F$6)","v":85.758839641505446}]
["ANAMET-S",3090061,"1/4\"","ZHLS conduit with black cover, Galvanised steel core, Polyolefin cover",30,14.037656450906157,{"$f":"F1135*(1-Elteq!$F$6)","v":14.037656450906157}]
["ANAMET-S",3090101,"5/16\"","ZHLS conduit with black cover, Galvanised steel core, Polyolefin cover",30,10.544500378410646,{"$f":"F1136*(1-Elteq!$F$6)","v":10.544500378410646}]
["ANAMET-S",3090103,"5/16\"","ZHLS conduit with black cover, Galvanised steel core, Polyolefin cover",10,10.544500378410646,{"$f":"F1137*(1-Elteq!$F$6)","v":10.544500378410646}]
["ANAMET-S",3090121,"3/8\"","ZHLS conduit with black cover, Galvanised steel core, Polyolefin cover",30,9.1323734554869311,{"$f":"F1138*(1-Elteq!$F$6)","v":9.1323734554869311}]
["ANAMET-S",3090123,"3/8\"","ZHLS conduit with black cover, Galvanised steel core, Polyolefin cover",10,9.1323734554869311,{"$f":"F1139*(1-Elteq!$F$6)","v":9.1323734554869311}]
["ANAMET-S",3090125,"3/8\"","ZHLS conduit with black cover, Galvanised steel core, Polyolefin cover",250,9.1323734554869311,{"$f":"F1140*(1-Elteq!$F$6)","v":9.1323734554869311}]
["ANAMET-S",3090161,"1/2\"","ZHLS conduit with black cover, Galvanised steel core, Polyolefin cover",30,11.585014953196543,{"$f":"F1141*(1-Elteq!$F$6)","v":11.585014953196543}]
["ANAMET-S",3090163,"1/2\"","ZHLS conduit with black cover, Galvanised steel core, Polyolefin cover",10,11.585014953196543,{"$f":"F1142*(1-Elteq!$F$6)","v":11.585014953196543}]
["ANAMET-S",3090165,"1/2\"","ZHLS conduit with black cover, Galvanised steel core, Polyolefin cover",150,11.585014953196543,{"$f":"F1143*(1-Elteq!$F$6)","v":11.585014953196543}]
["ANAMET-S",3090201,"3/4\"","ZHLS conduit with black cover, Galvanised steel core, Polyolefin cover",30,12.876367862975467,{"$f":"F1144*(1-Elteq!$F$6)","v":12.876367862975467}]
["ANAMET-S",3090203,"3/4\"","ZHLS conduit with black cover, Galvanised steel core, Polyolefin cover",10,12.876367862975467,{"$f":"F1145*(1-Elteq!$F$6)","v":12.876367862975467}]
["ANAMET-S",3090205,"3/4\"","ZHLS conduit with black cover, Galvanised steel core, Polyolefin cover",120,12.876367862975467,{"$f":"F1146*(1-Elteq!$F$6)","v":12.876367862975467}]
["ANAMET-S",3090261,"1\"","ZHLS conduit with black cover, Galvanised steel core, Polyolefin cover",30,16.806168444532915,{"$f":"F1147*(1-Elteq!$F$6)","v":16.806168444532915}]
["ANAMET-S",3090263,"1\"","ZHLS conduit with black cover, Galvanised steel core, Polyolefin cover",10,16.806168444532915,{"$f":"F1148*(1-Elteq!$F$6)","v":16.806168444532915}]
["ANAMET-S",3090265,"1\"","ZHLS conduit with black cover, Galvanised steel core, Polyolefin cover",90,16.806168444532915,{"$f":"F1149*(1-Elteq!$F$6)","v":16.806168444532915}]
["ANAMET-S",3090351,"1 1/4\"","ZHLS conduit with black cover, Galvanised steel core, Polyolefin cover",15,21.664999896434917,{"$f":"F1150*(1-Elteq!$F$6)","v":21.664999896434917}]
["ANAMET-S",3090355,"1 1/4\"","ZHLS conduit with black cover, Galvanised steel core, Polyolefin cover",60,21.664999896434917,{"$f":"F1151*(1-Elteq!$F$6)","v":21.664999896434917}]
["ANAMET-S",3090401,"1 1/2\"","ZHLS conduit with black cover, Galvanised steel core, Polyolefin cover",15,69.60299280621372,{"$f":"F1152*(1-Elteq!$F$6)","v":69.60299280621372}]
["ANAMET-S",3090405,"1 1/2\"","ZHLS conduit with black cover, Galvanised steel core, Polyolefin cover",45,69.60299280621372,{"$f":"F1153*(1-Elteq!$F$6)","v":69.60299280621372}]
["ANAMET-S",3090501,"2\"","ZHLS conduit with black cover, Galvanised steel core, Polyolefin cover",15,78.846849966142003,{"$f":"F1154*(1-Elteq!$F$6)","v":78.846849966142003}]
["ANAMET-S",3090505,"2\"","ZHLS conduit with black cover, Galvanised steel core, Polyolefin cover",22,78.846849966142003,{"$f":"F1155*(1-Elteq!$F$6)","v":78.846849966142003}]
["ANAMET-S",3480101,"5/16\"","HFX conduit with black cover, Galvanised steel core with TPU V0 cover",30,13.535979780920099,{"$f":"F1156*(1-Elteq!$F$6)","v":13.535979780920099}]
["ANAMET-S",3480121,"3/8\"","HFX conduit with black cover, Galvanised steel core with TPU V0 cover",30,11.715079275044781,{"$f":"F1157*(1-Elteq!$F$6)","v":11.715079275044781}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},3480161,"1/2\"","HFX conduit with black cover, Galvanised steel core with TPU V0 cover",30,14.864493925512807,{"$f":"F1158*(1-Elteq!$F$6)","v":14.864493925512807}]
["ANAMET-S",3480201,"3/4\"","HFX conduit with black cover, Galvanised steel core with TPU V0 cover",30,16.518168874726108,{"$f":"F1159*(1-Elteq!$F$6)","v":16.518168874726108}]
["ANAMET-S",3480261,"1\"","HFX conduit with black cover, Galvanised steel core with TPU V0 cover",30,23.569513180641245,{"$f":"F1160*(1-Elteq!$F$6)","v":23.569513180641245}]
["ANAMET-S",3480351,"1 1/4\"","HFX conduit with black cover, Galvanised steel core with TPU V0 cover",15,28.818537598087953,{"$f":"F1161*(1-Elteq!$F$6)","v":28.818537598087953}]
["ANAMET-S",3480401,"1 1/2\"","HFX conduit with black cover, Galvanised steel core with TPU V0 cover",15,92.475732834096561,{"$f":"F1162*(1-Elteq!$F$6)","v":92.475732834096561}]
["ANAMET-S",3480501,"2\"","HFX conduit with black cover, Galvanised steel core with TPU V0 cover",15,104.76681124875495,{"$f":"F1163*(1-Elteq!$F$6)","v":104.76681124875495}]
["ANAMET-S",3125121,"3/8\"","HTUA conduit with grey cover, Galvanised steel core with PVC cover",60,8.9465672814180213,{"$f":"F1164*(1-Elteq!$F$6)","v":8.9465672814180213}]
["ANAMET-S",3125161,"1/2\"","HTUA conduit with grey cover, Galvanised steel core with PVC cover",60,11.371337853017296,{"$f":"F1165*(1-Elteq!$F$6)","v":11.371337853017296}]
["ANAMET-S",3125201,"3/4\"","HTUA conduit with grey cover, Galvanised steel core with PVC cover",45,16.230169304919293,{"$f":"F1166*(1-Elteq!$F$6)","v":16.230169304919293}]
["ANAMET-S",3125261,"1\"","HTUA conduit with grey cover, Galvanised steel core with PVC cover",30,26.22654146982666,{"$f":"F1167*(1-Elteq!$F$6)","v":26.22654146982666}]
["ANAMET-S",3125351,"1.1/4\"","HTUA conduit with grey cover, Galvanised steel core with PVC cover",15,33.844594606651974,{"$f":"F1168*(1-Elteq!$F$6)","v":33.844594606651974}]
["ANAMET-S",3125401,"1 1/2\"","HTUA conduit with grey cover, Galvanised steel core with PVC cover",15,42.642516948814865,{"$f":"F1169*(1-Elteq!$F$6)","v":42.642516948814865}]
["ANAMET-S",3125501,"2\"","HTUA conduit with grey cover, Galvanised steel core with PVC cover",15,56.540818769169334,{"$f":"F1170*(1-Elteq!$F$6)","v":56.540818769169334}]
["ANAMET-S",3300122,"3/8\"","HTDL conduit with black cover, Galvanised steel core with PVC cover",60,8.9465672814180213,{"$f":"F1171*(1-Elteq!$F$6)","v":8.9465672814180213}]
["ANAMET-S",3300123,"3/8\"","HTDL conduit with black cover, Galvanised steel core with PVC cover",10,8.9465672814180213,{"$f":"F1172*(1-Elteq!$F$6)","v":8.9465672814180213}]
["ANAMET-S",3300125,"3/8\"","HTDL conduit with black cover, Galvanised steel core with PVC cover",150,8.9465672814180213,{"$f":"F1173*(1-Elteq!$F$6)","v":8.9465672814180213}]
["ANAMET-S",3300162,"1/2\"","HTDL conduit with black cover, Galvanised steel core with PVC cover",60,11.371337853017296,{"$f":"F1174*(1-Elteq!$F$6)","v":11.371337853017296}]
["ANAMET-S",3300163,"1/2\"","HTDL conduit with black cover, Galvanised steel core with PVC cover",10,11.371337853017296,{"$f":"F1175*(1-Elteq!$F$6)","v":11.371337853017296}]
["ANAMET-S",3300165,"1/2\"","HTDL conduit with black cover, Galvanised steel core with PVC cover",150,11.371337853017296,{"$f":"F1176*(1-Elteq!$F$6)","v":11.371337853017296}]
["ANAMET-S",3300202,"3/4\"","HTDL conduit with black cover, Galvanised steel core with PVC cover",45,16.230169304919293,{"$f":"F1177*(1-Elteq!$F$6)","v":16.230169304919293}]
["ANAMET-S",3300203,"3/4\"","HTDL conduit with black cover, Galvanised steel core with PVC cover",10,16.230169304919293,{"$f":"F1178*(1-Elteq!$F$6)","v":16.230169304919293}]
["ANAMET-S",3300205,"3/4\"","HTDL conduit with black cover, Galvanised steel core with PVC cover",120,16.230169304919293,{"$f":"F1179*(1-Elteq!$F$6)","v":16.230169304919293}]
["ANAMET-S",3300261,"1\"","HTDL conduit with black cover, Galvanised steel core with PVC cover",30,26.22654146982666,{"$f":"F1180*(1-Elteq!$F$6)","v":26.22654146982666}]
["ANAMET-S",3300263,"1\"","HTDL conduit with black cover, Galvanised steel core with PVC cover",10,26.22654146982666,{"$f":"F1181*(1-Elteq!$F$6)","v":26.22654146982666}]
["ANAMET-S",3300265,"1\"","HTDL conduit with black cover, Galvanised steel core with PVC cover",150,26.22654146982666,{"$f":"F1182*(1-Elteq!$F$6)","v":26.22654146982666}]
["ANAMET-S",3300351,"1 1/4\"","HTDL conduit with black cover, Galvanised steel core with PVC cover",15,33.853884915355415,{"$f":"F1183*(1-Elteq!$F$6)","v":33.853884915355415}]
["ANAMET-S",3300355,"1 1/4\"","HTDL conduit with black cover, Galvanised steel core with PVC cover",60,33.853884915355415,{"$f":"F1184*(1-Elteq!$F$6)","v":33.853884915355415}]
["ANAMET-S",3300401,"1 1/2\"","HTDL conduit with black cover, Galvanised steel core with PVC cover",15,42.642516948814865,{"$f":"F1185*(1-Elteq!$F$6)","v":42.642516948814865}]
["ANAMET-S",3300405,"1 1/2\"","HTDL conduit with black cover, Galvanised steel core with PVC cover",45,42.642516948814865,{"$f":"F1186*(1-Elteq!$F$6)","v":42.642516948814865}]
["ANAMET-S",3300501,"2\"","HTDL conduit with black cover, Galvanised steel core with PVC cover",15,56.540818769169334,{"$f":"F1187*(1-Elteq!$F$6)","v":56.540818769169334}]
["ANAMET-S",3300505,"2\"","HTDL conduit with black cover, Galvanised steel core with PVC cover",30,56.540818769169334,{"$f":"F1188*(1-Elteq!$F$6)","v":56.540818769169334}]
["ANAMET-S",3230161,"1/2\"","CW conduit with blue cover, Galvanised steel core with PVC cover",30,10.721016243776111,{"$f":"F1189*(1-Elteq!$F$6)","v":10.721016243776111}]
["ANAMET-S",3230201,"3/4\"","CW conduit with blue cover, Galvanised steel core with PVC cover",30,15.310428743278191,{"$f":"F1190*(1-Elteq!$F$6)","v":15.310428743278191}]
["ANAMET-S",3230261,"1\"","CW conduit with blue cover, Galvanised steel core with PVC cover",30,24.749382385978823,{"$f":"F1191*(1-Elteq!$F$6)","v":24.749382385978823}]
["ANAMET-S",3230351,"1 1/4\"","CW conduit with blue cover, Galvanised steel core with PVC cover",15,31.940081322445646,{"$f":"F1192*(1-Elteq!$F$6)","v":31.940081322445646}]
["ANAMET-S",3230401,"1 1/2\"","CW conduit with blue cover, Galvanised steel core with PVC cover",15,40.227036685919032,{"$f":"F1193*(1-Elteq!$F$6)","v":40.227036685919032}]
["ANAMET-S",3230501,"2\"","CW conduit with blue cover, Galvanised steel core with PVC cover",15,53.335662266480639,{"$f":"F1194*(1-Elteq!$F$6)","v":53.335662266480639}]
["ANAMET-S",3340121,"3/8\"","ZHUA conduit with black cover, Galvanised steel core with TPU V0 cover",30,18.673520493925462,{"$f":"F1195*(1-Elteq!$F$6)","v":18.673520493925462}]
["ANAMET-S",3340125,"3/8\"","ZHUA conduit with black cover, Galvanised steel core with TPU V0 cover",150,18.673520493925462,{"$f":"F1196*(1-Elteq!$F$6)","v":18.673520493925462}]
["ANAMET-S",3340161,"1/2\"","ZHUA conduit with black cover, Galvanised steel core with TPU V0 cover",30,21.692870822545252,{"$f":"F1197*(1-Elteq!$F$6)","v":21.692870822545252}]
["ANAMET-S",3340165,"1/2\"","ZHUA conduit with black cover, Galvanised steel core with TPU V0 cover",150,21.692870822545252,{"$f":"F1198*(1-Elteq!$F$6)","v":21.692870822545252}]
["ANAMET-S",3340201,"3/4\"","ZHUA conduit with black cover, Galvanised steel core with TPU V0 cover",30,28.493376793467363,{"$f":"F1199*(1-Elteq!$F$6)","v":28.493376793467363}]
["ANAMET-S",3340205,"3/4\"","ZHUA conduit with black cover, Galvanised steel core with TPU V0 cover",150,28.493376793467363,{"$f":"F1200*(1-Elteq!$F$6)","v":28.493376793467363}]
["ANAMET-S",3340261,"1 \"","ZHUA conduit with black cover, Galvanised steel core with TPU V0 cover",30,51.81205163911558,{"$f":"F1201*(1-Elteq!$F$6)","v":51.81205163911558}]
["ANAMET-S",3340265,"1 \"","ZHUA conduit with black cover, Galvanised steel core with TPU V0 cover",120,51.81205163911558,{"$f":"F1202*(1-Elteq!$F$6)","v":51.81205163911558}]
["ANAMET-S",3340351,"1 1/4 \"","ZHUA conduit with black cover, Galvanised steel core with TPU V0 cover",15,76.71007896434952,{"$f":"F1203*(1-Elteq!$F$6)","v":76.71007896434952}]
["ANAMET-S",3340355,"1 1/4 \"","ZHUA conduit with black cover, Galvanised steel core with TPU V0 cover",60,76.71007896434952,{"$f":"F1204*(1-Elteq!$F$6)","v":76.71007896434952}]
["ANAMET-S",3340401,"1 1/2\"","ZHUA conduit with black cover, Galvanised steel core with TPU V0 cover",15,111.02847931487723,{"$f":"F1205*(1-Elteq!$F$6)","v":111.02847931487723}]
["ANAMET-S",3340405,"1 1/2\"","ZHUA conduit with black cover, Galvanised steel core with TPU V0 cover",45,111.02847931487723,{"$f":"F1206*(1-Elteq!$F$6)","v":111.02847931487723}]
["ANAMET-S",3340501,"2\"","ZHUA conduit with black cover, Galvanised steel core with TPU V0 cover",15,143.68391440748817,{"$f":"F1207*(1-Elteq!$F$6)","v":143.68391440748817}]
["ANAMET-S",3340505,"2\"","ZHUA conduit with black cover, Galvanised steel core with TPU V0 cover",30,143.68391440748817,{"$f":"F1208*(1-Elteq!$F$6)","v":143.68391440748817}]
["ANAMET-S",3180061,"1/4\"","HCI conduit with black cover, Stainless steel 304 core with PVC cover",50,14.502171886078431,{"$f":"F1209*(1-Elteq!$F$6)","v":14.502171886078431}]
["ANAMET-S",3180101,"5/16\"","HCI conduit with black cover, Stainless steel 304 core with PVC cover",50,13.861140585540692,{"$f":"F1210*(1-Elteq!$F$6)","v":13.861140585540692}]
["ANAMET-S",3180103,"5/16\"","HCI conduit with black cover, Stainless steel 304 core with PVC cover",10,13.861140585540692,{"$f":"F1211*(1-Elteq!$F$6)","v":13.861140585540692}]
["ANAMET-S",3180121,"3/8\"","HCI conduit with black cover, Stainless steel 304 core with PVC cover",75,13.861140585540692,{"$f":"F1212*(1-Elteq!$F$6)","v":13.861140585540692}]
["ANAMET-S",3180123,"3/8\"","HCI conduit with black cover, Stainless steel 304 core with PVC cover",10,13.861140585540692,{"$f":"F1213*(1-Elteq!$F$6)","v":13.861140585540692}]
["ANAMET-S",3180161,"1/2\"","HCI conduit with black cover, Stainless steel 304 core with PVC cover",60,17.939586106353268,{"$f":"F1214*(1-Elteq!$F$6)","v":17.939586106353268}]
["ANAMET-S",3180163,"1/2\"","HCI conduit with black cover, Stainless steel 304 core with PVC cover",10,17.939586106353268,{"$f":"F1215*(1-Elteq!$F$6)","v":17.939586106353268}]
["ANAMET-S",3180201,"3/4\"","HCI conduit with black cover, Stainless steel 304 core with PVC cover",50,23.680996885082589,{"$f":"F1216*(1-Elteq!$F$6)","v":23.680996885082589}]
["ANAMET-S",3180203,"3/4\"","HCI conduit with black cover, Stainless steel 304 core with PVC cover",10,23.680996885082589,{"$f":"F1217*(1-Elteq!$F$6)","v":23.680996885082589}]
["ANAMET-S",3180261,"1\"","HCI conduit with black cover, Stainless steel 304 core with PVC cover",30,40.319939772953482,{"$f":"F1218*(1-Elteq!$F$6)","v":40.319939772953482}]
["ANAMET-S",3180263,"1\"","HCI conduit with black cover, Stainless steel 304 core with PVC cover",10,40.319939772953482,{"$f":"F1219*(1-Elteq!$F$6)","v":40.319939772953482}]
["ANAMET-S",3180351,"1 1/4\"","HCI conduit with black cover, Stainless steel 304 core with PVC cover",30,51.942115960963811,{"$f":"F1220*(1-Elteq!$F$6)","v":51.942115960963811}]
["ANAMET-S",3180353,"1 1/4\"","HCI conduit with black cover, Stainless steel 304 core with PVC cover",10,51.942115960963811,{"$f":"F1221*(1-Elteq!$F$6)","v":51.942115960963811}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},3180401,"1.1/2\"","HCI conduit with black cover, Stainless steel 304 core with PVC cover",15,126.11594064927272,{"$f":"F1222*(1-Elteq!$F$6)","v":126.11594064927272}]
["ANAMET-S",3180501,"2\"","HCI conduit with black cover, Stainless steel 304 core with PVC cover",15,175.30812523401664,{"$f":"F1223*(1-Elteq!$F$6)","v":175.30812523401664}]
["ANAMET-S",3580121,"3/8\"","HCI conduit with blue cover, Stainless steel 304 core with PVC cover",30,14.557913738299105,{"$f":"F1224*(1-Elteq!$F$6)","v":14.557913738299105}]
["ANAMET-S",3580161,"1/2\"","HCI conduit with blue cover, Stainless steel 304 core with PVC cover",30,18.840746050587484,{"$f":"F1225*(1-Elteq!$F$6)","v":18.840746050587484}]
["ANAMET-S",3580201,"3/4\"","HCI conduit with blue cover, Stainless steel 304 core with PVC cover",30,24.860866090420171,{"$f":"F1226*(1-Elteq!$F$6)","v":24.860866090420171}]
["ANAMET-S",3580261,"1\"","HCI conduit with blue cover, Stainless steel 304 core with PVC cover",30,42.335936761601161,{"$f":"F1227*(1-Elteq!$F$6)","v":42.335936761601161}]
["ANAMET-S",3580351,"1 1/4\"","HCI conduit with blue cover, Stainless steel 304 core with PVC cover",30,54.543402397928553,{"$f":"F1228*(1-Elteq!$F$6)","v":54.543402397928553}]
["ANAMET-S",3330061,"1/4\"","HFI conduit with black cover, Stainless steel 304 core with TPU cover",30,14.502171886078431,{"$f":"F1229*(1-Elteq!$F$6)","v":14.502171886078431}]
["ANAMET-S",3330101,"5/16\"","HFI conduit with black cover, Stainless steel 304 core with TPU cover",30,16.341653009360641,{"$f":"F1230*(1-Elteq!$F$6)","v":16.341653009360641}]
["ANAMET-S",3330103,"5/16\"","HFI conduit with black cover, Stainless steel 304 core with TPU cover",10,16.341653009360641,{"$f":"F1231*(1-Elteq!$F$6)","v":16.341653009360641}]
["ANAMET-S",3330121,"3/8\"","HFI conduit with black cover, Stainless steel 304 core with TPU cover",30,16.341653009360641,{"$f":"F1232*(1-Elteq!$F$6)","v":16.341653009360641}]
["ANAMET-S",3330123,"3/8\"","HFI conduit with black cover, Stainless steel 304 core with TPU cover",10,16.341653009360641,{"$f":"F1233*(1-Elteq!$F$6)","v":16.341653009360641}]
["ANAMET-S",3330161,"1/2\"","HFI conduit with black cover, Stainless steel 304 core with TPU cover",30,20.5594531607249,{"$f":"F1234*(1-Elteq!$F$6)","v":20.5594531607249}]
["ANAMET-S",3330163,"1/2\"","HFI conduit with black cover, Stainless steel 304 core with TPU cover",10,20.5594531607249,{"$f":"F1235*(1-Elteq!$F$6)","v":20.5594531607249}]
["ANAMET-S",3330201,"3/4\"","HFI conduit with black cover, Stainless steel 304 core with TPU cover",30,26.198670543716322,{"$f":"F1236*(1-Elteq!$F$6)","v":26.198670543716322}]
["ANAMET-S",3330203,"3/4\"","HFI conduit with black cover, Stainless steel 304 core with TPU cover",10,26.198670543716322,{"$f":"F1237*(1-Elteq!$F$6)","v":26.198670543716322}]
["ANAMET-S",3330261,"1\"","HFI conduit with black cover, Stainless steel 304 core with TPU cover",30,45.587544807807092,{"$f":"F1238*(1-Elteq!$F$6)","v":45.587544807807092}]
["ANAMET-S",3330263,"1\"","HFI conduit with black cover, Stainless steel 304 core with TPU cover",10,45.587544807807092,{"$f":"F1239*(1-Elteq!$F$6)","v":45.587544807807092}]
["ANAMET-S",3330351,"1 1/4\"","HFI conduit with black cover, Stainless steel 304 core with TPU cover",15,60.164039163513088,{"$f":"F1240*(1-Elteq!$F$6)","v":60.164039163513088}]
["ANAMET-S",3392121,"3/8\"","HFI conduit with blue cover, Stainless steel 304 core with TPU cover",30,17.159200175263845,{"$f":"F1241*(1-Elteq!$F$6)","v":17.159200175263845}]
["ANAMET-S",3392161,"1/2\"","HFI conduit with blue cover, Stainless steel 304 core with TPU cover",30,21.59067742680735,{"$f":"F1242*(1-Elteq!$F$6)","v":21.59067742680735}]
["ANAMET-S",3392201,"3/4\"","HFI conduit with blue cover, Stainless steel 304 core with TPU cover",30,27.517894379605583,{"$f":"F1243*(1-Elteq!$F$6)","v":27.517894379605583}]
["ANAMET-S",3392261,"1\"","HFI conduit with blue cover, Stainless steel 304 core with TPU cover",30,47.863670440151239,{"$f":"F1244*(1-Elteq!$F$6)","v":47.863670440151239}]
["ANAMET-S",3392351,"1 1/4\"","HFI conduit with blue cover, Stainless steel 304 core with TPU cover",15,63.174099183429433,{"$f":"F1245*(1-Elteq!$F$6)","v":63.174099183429433}]
["ANAMET-S",3190121,"3/8\"","HCI-316 conduit with black cover, Stainless steel 316 core with PVC cover",30,15.254686891057519,{"$f":"F1246*(1-Elteq!$F$6)","v":15.254686891057519}]
["ANAMET-S",3190123,"3/8\"","HCI-316 conduit with black cover, Stainless steel 316 core with PVC cover",10,15.254686891057519,{"$f":"F1247*(1-Elteq!$F$6)","v":15.254686891057519}]
["ANAMET-S",3190161,"1/2\"","HCI-316 conduit with black cover, Stainless steel 316 core with PVC cover",30,19.741905994821696,{"$f":"F1248*(1-Elteq!$F$6)","v":19.741905994821696}]
["ANAMET-S",3190163,"1/2\"","HCI-316 conduit with black cover, Stainless steel 316 core with PVC cover",10,19.741905994821696,{"$f":"F1249*(1-Elteq!$F$6)","v":19.741905994821696}]
["ANAMET-S",3190201,"3/4\"","HCI-316 conduit with black cover, Stainless steel 316 core with PVC cover",30,26.059315913164642,{"$f":"F1250*(1-Elteq!$F$6)","v":26.059315913164642}]
["ANAMET-S",3190203,"3/4\"","HCI-316 conduit with black cover, Stainless steel 316 core with PVC cover",10,26.059315913164642,{"$f":"F1251*(1-Elteq!$F$6)","v":26.059315913164642}]
["ANAMET-S",3190261,"1\"","HCI-316 conduit with black cover, Stainless steel 316 core with PVC cover",30,44.351933750248833,{"$f":"F1252*(1-Elteq!$F$6)","v":44.351933750248833}]
["ANAMET-S",3190263,"1\"","HCI-316 conduit with black cover, Stainless steel 316 core with PVC cover",10,44.351933750248833,{"$f":"F1253*(1-Elteq!$F$6)","v":44.351933750248833}]
["ANAMET-S",3400121,"3/8\"","HCXI conduit with black cover, Stainless steel 304 core with TPE cover",30,22.333902123082993,{"$f":"F1254*(1-Elteq!$F$6)","v":22.333902123082993}]
["ANAMET-S",3400123,"3/8\"","HCXI conduit with black cover, Stainless steel 304 core with TPE cover",10,22.333902123082993,{"$f":"F1255*(1-Elteq!$F$6)","v":22.333902123082993}]
["ANAMET-S",3400161,"1/2\"","HCXI conduit with black cover, Stainless steel 304 core with TPE cover",30,25.64125202150959,{"$f":"F1256*(1-Elteq!$F$6)","v":25.64125202150959}]
["ANAMET-S",3400163,"1/2\"","HCXI conduit with black cover, Stainless steel 304 core with TPE cover",10,25.64125202150959,{"$f":"F1257*(1-Elteq!$F$6)","v":25.64125202150959}]
["ANAMET-S",3400201,"3/4\"","HCXI conduit with black cover, Stainless steel 304 core with TPE cover",30,35.507559864568712,{"$f":"F1258*(1-Elteq!$F$6)","v":35.507559864568712}]
["ANAMET-S",3400203,"3/4\"","HCXI conduit with black cover, Stainless steel 304 core with TPE cover",10,35.507559864568712,{"$f":"F1259*(1-Elteq!$F$6)","v":35.507559864568712}]
["ANAMET-S",3400261,"1\"","HCXI conduit with black cover, Stainless steel 304 core with TPE cover",30,46.293608269268944,{"$f":"F1260*(1-Elteq!$F$6)","v":46.293608269268944}]
["ANAMET-S",3400263,"1\"","HCXI conduit with black cover, Stainless steel 304 core with TPE cover",10,46.293608269268944,{"$f":"F1261*(1-Elteq!$F$6)","v":46.293608269268944}]
["ANAMET-S",3400351,"1.1/4\"","HCXI conduit with black cover, Stainless steel 304 core with TPE cover",15,60.563522437761236,{"$f":"F1262*(1-Elteq!$F$6)","v":60.563522437761236}]
["ANAMET-S",2980126,"NPT 1/2\"","Aluminium fittings for Sealtite EFL, Straight fixed with male thread, IP 68",25,15.877137574188366,{"$f":"F1263*(1-Elteq!$F$6)","v":15.877137574188366}]
["ANAMET-S",2980166,"NPT 1/2\"","Aluminium fittings for Sealtite EFL, Straight fixed with male thread, IP 68",25,17.921005488946378,{"$f":"F1264*(1-Elteq!$F$6)","v":17.921005488946378}]
["ANAMET-S",2980206,"NPT 3/4\"","Aluminium fittings for Sealtite EFL, Straight fixed with male thread, IP 68",25,18.924358828918493,{"$f":"F1265*(1-Elteq!$F$6)","v":18.924358828918493}]
["ANAMET-S",2980266,"NPT 1\"","Aluminium fittings for Sealtite EFL, Straight fixed with male thread, IP 68",5,35.526140481975609,{"$f":"F1266*(1-Elteq!$F$6)","v":35.526140481975609}]
["ANAMET-S",2980356,"NPT 1 1/4\"","Aluminium fittings for Sealtite EFL, Straight fixed with male thread, IP 68",5,63.954485114518853,{"$f":"F1267*(1-Elteq!$F$6)","v":63.954485114518853}]
["ANAMET-S",2980406,"NPT 1 1/2\"","Aluminium fittings for Sealtite EFL, Straight fixed with male thread, IP 68",2,87.152385947022267,{"$f":"F1268*(1-Elteq!$F$6)","v":87.152385947022267}]
["ANAMET-S",2980506,"NPT 2\"","Aluminium fittings for Sealtite EFL, Straight fixed with male thread, IP 68",1,104.01429624377586,{"$f":"F1269*(1-Elteq!$F$6)","v":104.01429624377586}]
["ANAMET-S",2989126,"NPT 1/2\"","Aluminium fittings for Sealtite EFL, 90° elbow fixed with male thread, IP 68",25,17.224232336187963,{"$f":"F1270*(1-Elteq!$F$6)","v":17.224232336187963}]
["ANAMET-S",2989166,"NPT 1/2\"","Aluminium fittings for Sealtite EFL, 90° elbow fixed with male thread, IP 68",25,18.543456172077228,{"$f":"F1271*(1-Elteq!$F$6)","v":18.543456172077228}]
["ANAMET-S",2989206,"NPT 3/4\"","Aluminium fittings for Sealtite EFL, 90° elbow fixed with male thread, IP 68",10,44.853610420234894,{"$f":"F1272*(1-Elteq!$F$6)","v":44.853610420234894}]
["ANAMET-S",2989266,"NPT 1\"","Aluminium fittings for Sealtite EFL, 90° elbow fixed with male thread, IP 68",5,52.183663987253396,{"$f":"F1273*(1-Elteq!$F$6)","v":52.183663987253396}]
["ANAMET-S",2989356,"NPT 1 1/4\"","Aluminium fittings for Sealtite EFL, 90° elbow fixed with male thread, IP 68",5,100.47468862776313,{"$f":"F1274*(1-Elteq!$F$6)","v":100.47468862776313}]
["ANAMET-S",2989406,"NPT 1 1/2\"","Aluminium fittings for Sealtite EFL, 90° elbow fixed with male thread, IP 68",2,152.63048168890617,{"$f":"F1275*(1-Elteq!$F$6)","v":152.63048168890617}]
["ANAMET-S",2989506,"NPT 2\"","Aluminium fittings for Sealtite EFL, 90° elbow fixed with male thread, IP 68",1,285.84421818761126,{"$f":"F1276*(1-Elteq!$F$6)","v":285.84421818761126}]
["ANAMET-S",3240121,"3/8\"","EFL conduit with grey cover, Aluminium steel core with PVC cover",30,6.949150910177238,{"$f":"F1277*(1-Elteq!$F$6)","v":6.949150910177238}]
["ANAMET-S",3240161,"1/2\"","EFL conduit with grey cover, Aluminium steel core with PVC cover",30,7.7574077673769963,{"$f":"F1278*(1-Elteq!$F$6)","v":7.7574077673769963}]
["ANAMET-S",3240201,"3/4\"","EFL conduit with grey cover, Aluminium steel core with PVC cover",30,9.8755981517625724,{"$f":"F1279*(1-Elteq!$F$6)","v":9.8755981517625724}]
["ANAMET-S",3240261,"1\"","EFL conduit with grey cover, Aluminium steel core with PVC cover",30,14.130559537940611,{"$f":"F1280*(1-Elteq!$F$6)","v":14.130559537940611}]
["ANAMET-S",3240351,"1 1/4\"","EFL conduit with grey cover, Aluminium steel core with PVC cover",15,19.723325377414806,{"$f":"F1281*(1-Elteq!$F$6)","v":19.723325377414806}]
["ANAMET-S",3240401,"1 1/2\"","EFL conduit with grey cover, Aluminium steel core with PVC cover",15,27.044088635729864,{"$f":"F1282*(1-Elteq!$F$6)","v":27.044088635729864}]
["ANAMET-S",3240501,"2\"","EFL conduit with grey cover, Aluminium steel core with PVC cover",15,35.0151735032861,{"$f":"F1283*(1-Elteq!$F$6)","v":35.0151735032861}]
["ANAMET-S",3040121,"3/8\"","SHIELDTITE conduit with grey cover, Bronze metal core with PVC cover",30,63.31345381398112,{"$f":"F1284*(1-Elteq!$F$6)","v":63.31345381398112}]
["ANAMET-S",3040125,"3/8\"","SHIELDTITE conduit with grey cover, Bronze metal core with PVC cover",250,63.31345381398112,{"$f":"F1285*(1-Elteq!$F$6)","v":63.31345381398112}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},3040161,"1/2\"","SHIELDTITE conduit with grey cover, Bronze metal core with PVC cover",30,69.045574284006975,{"$f":"F1286*(1-Elteq!$F$6)","v":69.045574284006975}]
["ANAMET-S",3040165,"1/2\"","SHIELDTITE conduit with grey cover, Bronze metal core with PVC cover",150,69.045574284006975,{"$f":"F1287*(1-Elteq!$F$6)","v":69.045574284006975}]
["ANAMET-S",3040201,"3/4\"","SHIELDTITE conduit with grey cover, Bronze metal core with PVC cover",30,91.816120916151903,{"$f":"F1288*(1-Elteq!$F$6)","v":91.816120916151903}]
["ANAMET-S",3040203,"3/4\"","SHIELDTITE conduit with grey cover, Bronze metal core with PVC cover",10,91.816120916151903,{"$f":"F1289*(1-Elteq!$F$6)","v":91.816120916151903}]
["ANAMET-S",3040205,"3/4\"","SHIELDTITE conduit with grey cover, Bronze metal core with PVC cover",120,91.816120916151903,{"$f":"F1290*(1-Elteq!$F$6)","v":91.816120916151903}]
["ANAMET-S",3040261,"1\"","SHIELDTITE conduit with grey cover, Bronze metal core with PVC cover",30,108.87312769567787,{"$f":"F1291*(1-Elteq!$F$6)","v":108.87312769567787}]
["ANAMET-S",3040265,"1\"","SHIELDTITE conduit with grey cover, Bronze metal core with PVC cover",90,108.87312769567787,{"$f":"F1292*(1-Elteq!$F$6)","v":108.87312769567787}]
["ANAMET-S",3040351,"1 1/4\"","SHIELDTITE conduit with grey cover, Bronze metal core with PVC cover",15,161.88362915753791,{"$f":"F1293*(1-Elteq!$F$6)","v":161.88362915753791}]
["ANAMET-S",3040355,"1 1/4\"","SHIELDTITE conduit with grey cover, Bronze metal core with PVC cover",60,161.88362915753791,{"$f":"F1294*(1-Elteq!$F$6)","v":161.88362915753791}]
["ANAMET-S",3040401,"1 1/2\"","SHIELDTITE conduit with grey cover, Bronze metal core with PVC cover",15,209.60794496713748,{"$f":"F1295*(1-Elteq!$F$6)","v":209.60794496713748}]
["ANAMET-S",3040405,"1 1/2\"","SHIELDTITE conduit with grey cover, Bronze metal core with PVC cover",45,209.60794496713748,{"$f":"F1296*(1-Elteq!$F$6)","v":209.60794496713748}]
["ANAMET-S",3040501,"2\"","SHIELDTITE conduit with grey cover, Bronze metal core with PVC cover",15,231.66313782911712,{"$f":"F1297*(1-Elteq!$F$6)","v":231.66313782911712}]
["ANAMET-S",3040505,"2\"","SHIELDTITE conduit with grey cover, Bronze metal core with PVC cover",30,231.66313782911712,{"$f":"F1298*(1-Elteq!$F$6)","v":231.66313782911712}]
["ANAMET-S",3042121,"3/8\"","SHIELDTITE Z1 conduit grey cover, Bronze metal core with TPU V0 cover",30,75.97614457677733,{"$f":"F1299*(1-Elteq!$F$6)","v":75.97614457677733}]
["ANAMET-S",3042161,"1/2\"","SHIELDTITE Z1 conduit grey cover, Bronze metal core with TPU V0 cover",30,82.850973017327021,{"$f":"F1300*(1-Elteq!$F$6)","v":82.850973017327021}]
["ANAMET-S",3042201,"3/4\"","SHIELDTITE Z1 conduit grey cover, Bronze metal core with TPU V0 cover",30,110.18306122286367,{"$f":"F1301*(1-Elteq!$F$6)","v":110.18306122286367}]
["ANAMET-S",3042261,"1\"","SHIELDTITE Z1 conduit grey cover, Bronze metal core with TPU V0 cover",30,130.64961129655413,{"$f":"F1302*(1-Elteq!$F$6)","v":130.64961129655413}]
["ANAMET-S",3042351,"1 1/4\"","SHIELDTITE Z1 conduit grey cover, Bronze metal core with TPU V0 cover",15,194.26035498904548,{"$f":"F1303*(1-Elteq!$F$6)","v":194.26035498904548}]
["ANAMET-S",3042401,"1 1/2\"","SHIELDTITE Z1 conduit grey cover, Bronze metal core with TPU V0 cover",15,251.52581783708357,{"$f":"F1304*(1-Elteq!$F$6)","v":251.52581783708357}]
["ANAMET-S",3042501,"2\"","SHIELDTITE Z1 conduit grey cover, Bronze metal core with TPU V0 cover",15,277.99390733319984,{"$f":"F1305*(1-Elteq!$F$6)","v":277.99390733319984}]
["ANAMET-S",3410121,"3/8\"","FG conduit with white cover, Galvanised steel core with PVC cover",30,8.9001157379007925,{"$f":"F1306*(1-Elteq!$F$6)","v":8.9001157379007925}]
["ANAMET-S",3410161,"1/2\"","FG conduit with white cover, Galvanised steel core with PVC cover",30,11.139080135431161,{"$f":"F1307*(1-Elteq!$F$6)","v":11.139080135431161}]
["ANAMET-S",3410201,"3/4\"","FG conduit with white cover, Galvanised steel core with PVC cover",30,11.919466066520581,{"$f":"F1308*(1-Elteq!$F$6)","v":11.919466066520581}]
["ANAMET-S",3410261,"1\"","FG conduit with white cover, Galvanised steel core with PVC cover",30,16.174427452698623,{"$f":"F1309*(1-Elteq!$F$6)","v":16.174427452698623}]
["ANAMET-S",3410351,"1 1/4\"","FG conduit with white cover, Galvanised steel core with PVC cover",15,23.588093798048138,{"$f":"F1310*(1-Elteq!$F$6)","v":23.588093798048138}]
["ANAMET-S",3410401,"1 1/2\"","FG conduit with white cover, Galvanised steel core with PVC cover",15,33.02704744074876,{"$f":"F1311*(1-Elteq!$F$6)","v":33.02704744074876}]
["ANAMET-S",3410501,"2\"","FG conduit with white cover, Galvanised steel core with PVC cover",15,40.375681625174167,{"$f":"F1312*(1-Elteq!$F$6)","v":40.375681625174167}]
["ANAMET-S",3520121,"3/8\"","FG conduit with blue cover, Galvanised steel core with PVC cover",30,8.9001157379007925,{"$f":"F1313*(1-Elteq!$F$6)","v":8.9001157379007925}]
["ANAMET-S",3520161,"1/2\"","FG conduit with blue cover, Galvanised steel core with PVC cover",30,11.139080135431161,{"$f":"F1314*(1-Elteq!$F$6)","v":11.139080135431161}]
["ANAMET-S",3520201,"3/4\"","FG conduit with blue cover, Galvanised steel core with PVC cover",30,11.919466066520581,{"$f":"F1315*(1-Elteq!$F$6)","v":11.919466066520581}]
["ANAMET-S",3520261,"1\"","FG conduit with blue cover, Galvanised steel core with PVC cover",30,16.174427452698623,{"$f":"F1316*(1-Elteq!$F$6)","v":16.174427452698623}]
["ANAMET-S",3520351,"1 1/4\"","FG conduit with blue cover, Galvanised steel core with PVC cover",15,23.588093798048138,{"$f":"F1317*(1-Elteq!$F$6)","v":23.588093798048138}]
["ANAMET-S",3520401,"1 1/2\"","FG conduit with blue cover, Galvanised steel core with PVC cover",15,33.02704744074876,{"$f":"F1318*(1-Elteq!$F$6)","v":33.02704744074876}]
["ANAMET-S",3520501,"2\"","FG conduit with blue cover, Galvanised steel core with PVC cover",15,40.375681625174167,{"$f":"F1319*(1-Elteq!$F$6)","v":40.375681625174167}]
["ANAMET-S",3280121,"3/8\"","NWC conduit with black cover, Galvanised steel core with PE cover",30,283.01067403306041,{"$f":"F1320*(1-Elteq!$F$6)","v":283.01067403306041}]
["ANAMET-S",3280161,"1/2\"","NWC conduit with black cover, Galvanised steel core with PE cover",30,345.7945802509451,{"$f":"F1321*(1-Elteq!$F$6)","v":345.7945802509451}]
["ANAMET-S",3280201,"3/4\"","NWC conduit with black cover, Galvanised steel core with PE cover",30,457.24112345747739,{"$f":"F1322*(1-Elteq!$F$6)","v":457.24112345747739}]
["ANAMET-S",3280261,"1\"","NWC conduit with black cover, Galvanised steel core with PE cover",30,649.06741756622012,{"$f":"F1323*(1-Elteq!$F$6)","v":649.06741756622012}]
["ANAMET-S",3280351,"1 1/4\"","NWC conduit with black cover, Galvanised steel core with PE cover",15,821.25399907587916,{"$f":"F1324*(1-Elteq!$F$6)","v":821.25399907587916}]
["ANAMET-S",3280401,"1 1/2\"","NWC conduit with black cover, Galvanised steel core with PE cover",15,931.63215678151505,{"$f":"F1325*(1-Elteq!$F$6)","v":931.63215678151505}]
["ANAMET-S",3280501,"2\"","NWC conduit with black cover, Galvanised steel core with PE cover",15,1145.773772395934,{"$f":"F1326*(1-Elteq!$F$6)","v":1145.773772395934}]
["ANAMET-S",3500121,"3/8\"","AS conduit with black cover, Galvanised steel core with PVC cover",30,7.9432139414459062,{"$f":"F1327*(1-Elteq!$F$6)","v":7.9432139414459062}]
["ANAMET-S",3500161,"1/2\"","AS conduit with black cover, Galvanised steel core with PVC cover",30,9.2438571599282771,{"$f":"F1328*(1-Elteq!$F$6)","v":9.2438571599282771}]
["ANAMET-S",3500201,"3/4\"","AS conduit with black cover, Galvanised steel core with PVC cover",30,13.285141445927071,{"$f":"F1329*(1-Elteq!$F$6)","v":13.285141445927071}]
["ANAMET-S",3500261,"1\"","AS conduit with black cover, Galvanised steel core with PVC cover",30,19.323842103166648,{"$f":"F1330*(1-Elteq!$F$6)","v":19.323842103166648}]
["ANAMET-S",3500351,"1 1/4\"","AS conduit with black cover, Galvanised steel core with PVC cover",15,24.758672694682264,{"$f":"F1331*(1-Elteq!$F$6)","v":24.758672694682264}]
["ANAMET-S",3500401,"1 1/2\"","AS conduit with black cover, Galvanised steel core with PVC cover",15,41.667034534953082,{"$f":"F1332*(1-Elteq!$F$6)","v":41.667034534953082}]
["ANAMET-S",3500501,"2\"","AS conduit with black cover, Galvanised steel core with PVC cover",15,53.605081218880564,{"$f":"F1333*(1-Elteq!$F$6)","v":53.605081218880564}]
["ANAMET-S",7100111,"PG 11","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",10,2.8428344632543241,{"$f":"F1334*(1-Elteq!$F$6)","v":2.8428344632543241}]
["ANAMET-S",7100131,"PG 13,5","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",10,2.8521247719577696,{"$f":"F1335*(1-Elteq!$F$6)","v":2.8521247719577696}]
["ANAMET-S",7100161,"PG 16","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",10,3.3630917506472726,{"$f":"F1336*(1-Elteq!$F$6)","v":3.3630917506472726}]
["ANAMET-S",7100211,"PG 21","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",5,5.1003794781915825,{"$f":"F1337*(1-Elteq!$F$6)","v":5.1003794781915825}]
["ANAMET-S",7100291,"PG 29","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",5,8.3055359808802809,{"$f":"F1338*(1-Elteq!$F$6)","v":8.3055359808802809}]
["ANAMET-S",7100361,"PG 36","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",2,12.959980641306478,{"$f":"F1339*(1-Elteq!$F$6)","v":12.959980641306478}]
["ANAMET-S",7100421,"PG 42","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",2,17.939586106353268,{"$f":"F1340*(1-Elteq!$F$6)","v":17.939586106353268}]
["ANAMET-S",7100481,"PG 48","Compact fittings for Sealtite, Straight fixed with male thread, IP 67","-",25.650542330213035,{"$f":"F1341*(1-Elteq!$F$6)","v":25.650542330213035}]
["ANAMET-S",7109111,"PG 11","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67","-",5.2304438000398186,{"$f":"F1342*(1-Elteq!$F$6)","v":5.2304438000398186}]
["ANAMET-S",7109131,"PG 13,5","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67","-",5.3976693567018375,{"$f":"F1343*(1-Elteq!$F$6)","v":5.3976693567018375}]
["ANAMET-S",7109161,"PG 16","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67","-",6.3917323879705075,{"$f":"F1344*(1-Elteq!$F$6)","v":6.3917323879705075}]
["ANAMET-S",7109211,"PG 21","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67","-",9.364631173073068,{"$f":"F1345*(1-Elteq!$F$6)","v":9.364631173073068}]
["ANAMET-S",7109291,"PG 29","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67","-",17.493651288587884,{"$f":"F1346*(1-Elteq!$F$6)","v":17.493651288587884}]
["ANAMET-S",7109361,"PG 36","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67","-",27.685119936267604,{"$f":"F1347*(1-Elteq!$F$6)","v":27.685119936267604}]
["ANAMET-S",7109421,"PG 42","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67","-",37.309879753037144,{"$f":"F1348*(1-Elteq!$F$6)","v":37.309879753037144}]
["ANAMET-S",7109481,"PG 48","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67","-",58.129461557458519,{"$f":"F1349*(1-Elteq!$F$6)","v":58.129461557458519}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},7120140,"M20 x 1,5","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",10,3.9762521250746765,{"$f":"F1350*(1-Elteq!$F$6)","v":3.9762521250746765}]
["ANAMET-S",7120150,"M16 x 1,5","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",10,3.7254137900816469,{"$f":"F1351*(1-Elteq!$F$6)","v":3.7254137900816469}]
["ANAMET-S",7120161,"M16 x 1,5","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",10,2.7963829197370966,{"$f":"F1352*(1-Elteq!$F$6)","v":2.7963829197370966}]
["ANAMET-S",7120171,"M20 x 1,5","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",10,3.047221254730125,{"$f":"F1353*(1-Elteq!$F$6)","v":3.047221254730125}]
["ANAMET-S",7120201,"M20 x 1,5","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",10,3.2237371200955898,{"$f":"F1354*(1-Elteq!$F$6)","v":3.2237371200955898}]
["ANAMET-S",7120251,"M25 x 1,5","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",5,4.9981860824536808,{"$f":"F1355*(1-Elteq!$F$6)","v":4.9981860824536808}]
["ANAMET-S",7120321,"M32 x 1,5","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",5,7.9617945588527972,{"$f":"F1356*(1-Elteq!$F$6)","v":7.9617945588527972}]
["ANAMET-S",7120401,"M40 x 1,5","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",2,12.839206628161687,{"$f":"F1357*(1-Elteq!$F$6)","v":12.839206628161687}]
["ANAMET-S",7120501,"M50 x 1,5","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",2,18.023198884684277,{"$f":"F1358*(1-Elteq!$F$6)","v":18.023198884684277}]
["ANAMET-S",7120631,"M63 x 1,5","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",2,25.827058195578502,{"$f":"F1359*(1-Elteq!$F$6)","v":25.827058195578502}]
["ANAMET-S",7124140,"M20 x 1,5","Compact fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,7.2371504799840478,{"$f":"F1360*(1-Elteq!$F$6)","v":7.2371504799840478}]
["ANAMET-S",7124150,"M16 x 1,5","Compact fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,6.3081196096394976,{"$f":"F1361*(1-Elteq!$F$6)","v":6.3081196096394976}]
["ANAMET-S",7124161,"M16 x 1,5","Compact fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,5.0260570085640177,{"$f":"F1362*(1-Elteq!$F$6)","v":5.0260570085640177}]
["ANAMET-S",7124171,"M20 x 1,5","Compact fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,5.9086363353913409,{"$f":"F1363*(1-Elteq!$F$6)","v":5.9086363353913409}]
["ANAMET-S",7124201,"M20 x 1,5","Compact fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,5.9922491137223508,{"$f":"F1364*(1-Elteq!$F$6)","v":5.9922491137223508}]
["ANAMET-S",7124251,"M25 x 1,5","Compact fittings for Sealtite, 45° elbow fixed with male thread, IP 67",5,9.4761148775144139,{"$f":"F1365*(1-Elteq!$F$6)","v":9.4761148775144139}]
["ANAMET-S",7124321,"M32 x 1,5","Compact fittings for Sealtite, 45° elbow fixed with male thread, IP 67",5,17.252103262298302,{"$f":"F1366*(1-Elteq!$F$6)","v":17.252103262298302}]
["ANAMET-S",7129140,"M20 x 1,5","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,6.8376672057358912,{"$f":"F1367*(1-Elteq!$F$6)","v":6.8376672057358912}]
["ANAMET-S",7129150,"M16 x 1,5","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,5.9550878789085679,{"$f":"F1368*(1-Elteq!$F$6)","v":5.9550878789085679}]
["ANAMET-S",7129161,"M16 x 1,5","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,5.0260570085640177,{"$f":"F1369*(1-Elteq!$F$6)","v":5.0260570085640177}]
["ANAMET-S",7129171,"M20 x 1,5","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,5.9086363353913409,{"$f":"F1370*(1-Elteq!$F$6)","v":5.9086363353913409}]
["ANAMET-S",7129201,"M20 x 1,5","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,5.9922491137223508,{"$f":"F1371*(1-Elteq!$F$6)","v":5.9922491137223508}]
["ANAMET-S",7129251,"M25 x 1,5","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",5,9.4761148775144139,{"$f":"F1372*(1-Elteq!$F$6)","v":9.4761148775144139}]
["ANAMET-S",7129321,"M32 x 1,5","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",5,17.252103262298302,{"$f":"F1373*(1-Elteq!$F$6)","v":17.252103262298302}]
["ANAMET-S",7129401,"M40 x 1,5","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,27.685119936267604,{"$f":"F1374*(1-Elteq!$F$6)","v":27.685119936267604}]
["ANAMET-S",7129501,"M50 x 1,5","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,37.309879753037144,{"$f":"F1375*(1-Elteq!$F$6)","v":37.309879753037144}]
["ANAMET-S",7129631,"M63 x 1,5","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,56.011271173072949,{"$f":"F1376*(1-Elteq!$F$6)","v":56.011271173072949}]
["ANAMET-S",7140121,"NPT 1/2\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",10,2.9450278589922245,{"$f":"F1377*(1-Elteq!$F$6)","v":2.9450278589922245}]
["ANAMET-S",7140122,"NPT 1/2\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",10,3.1587049591714713,{"$f":"F1378*(1-Elteq!$F$6)","v":3.1587049591714713}]
["ANAMET-S",7140161,"NPT 1/2\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",10,3.3723820593507181,{"$f":"F1379*(1-Elteq!$F$6)","v":3.3723820593507181}]
["ANAMET-S",7140162,"NPT 1/2\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",10,3.5860591595299645,{"$f":"F1380*(1-Elteq!$F$6)","v":3.5860591595299645}]
["ANAMET-S",7140201,"NPT 3/4\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",5,4.7287671300537619,{"$f":"F1381*(1-Elteq!$F$6)","v":4.7287671300537619}]
["ANAMET-S",7140202,"NPT 3/4\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",5,5.0725085520812456,{"$f":"F1382*(1-Elteq!$F$6)","v":5.0725085520812456}]
["ANAMET-S",7140261,"NPT 1\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",5,8.3148262895837259,{"$f":"F1383*(1-Elteq!$F$6)","v":8.3148262895837259}]
["ANAMET-S",7140262,"NPT 1\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",5,8.8072126508663384,{"$f":"F1384*(1-Elteq!$F$6)","v":8.8072126508663384}]
["ANAMET-S",7140351,"NPT 1.1/4\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",2,13.526689472216654,{"$f":"F1385*(1-Elteq!$F$6)","v":13.526689472216654}]
["ANAMET-S",7140352,"NPT 1.1/4\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",2,14.353526946823303,{"$f":"F1386*(1-Elteq!$F$6)","v":14.353526946823303}]
["ANAMET-S",7140401,"NPT 1.1/2\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",2,19.37029364668388,{"$f":"F1387*(1-Elteq!$F$6)","v":19.37029364668388}]
["ANAMET-S",7140402,"NPT 1.1/2\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",2,20.40151791276633,{"$f":"F1388*(1-Elteq!$F$6)","v":20.40151791276633}]
["ANAMET-S",7140501,"NPT 2\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",2,30.890276438956299,{"$f":"F1389*(1-Elteq!$F$6)","v":30.890276438956299}]
["ANAMET-S",7140502,"NPT 2\"","Compact fittings for Sealtite, Straight fixed with male thread, IP 67",2,32.358145214100688,{"$f":"F1390*(1-Elteq!$F$6)","v":32.358145214100688}]
["ANAMET-S",7144121,"NPT 1/2\"","Compact fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,5.4719918263294023,{"$f":"F1391*(1-Elteq!$F$6)","v":5.4719918263294023}]
["ANAMET-S",7144161,"NPT 1/2\"","Compact fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,6.5125064011152984,{"$f":"F1392*(1-Elteq!$F$6)","v":6.5125064011152984}]
["ANAMET-S",7144201,"NPT 3/4\"","Compact fittings for Sealtite, 45° elbow fixed with male thread, IP 67",5,9.3088893208523942,{"$f":"F1393*(1-Elteq!$F$6)","v":9.3088893208523942}]
["ANAMET-S",7144261,"NPT 1\"","Compact fittings for Sealtite, 45° elbow fixed with male thread, IP 67",5,17.252103262298302,{"$f":"F1394*(1-Elteq!$F$6)","v":17.252103262298302}]
["ANAMET-S",7149121,"NPT 1/2\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,5.4719918263294023,{"$f":"F1395*(1-Elteq!$F$6)","v":5.4719918263294023}]
["ANAMET-S",7149122,"NPT 1/2\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,5.6856689265086482,{"$f":"F1396*(1-Elteq!$F$6)","v":5.6856689265086482}]
["ANAMET-S",7149161,"NPT 1/2\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,6.5125064011152984,{"$f":"F1397*(1-Elteq!$F$6)","v":6.5125064011152984}]
["ANAMET-S",7149162,"NPT 1/2\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,6.7261835012945452,{"$f":"F1398*(1-Elteq!$F$6)","v":6.7261835012945452}]
["ANAMET-S",7149201,"NPT 3/4\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",5,9.3088893208523942,{"$f":"F1399*(1-Elteq!$F$6)","v":9.3088893208523942}]
["ANAMET-S",7149202,"NPT 3/4\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",5,9.6526307428798805,{"$f":"F1400*(1-Elteq!$F$6)","v":9.6526307428798805}]
["ANAMET-S",7149261,"NPT 1\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",5,17.252103262298302,{"$f":"F1401*(1-Elteq!$F$6)","v":17.252103262298302}]
["ANAMET-S",7149262,"NPT 1\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",5,17.744489623580915,{"$f":"F1402*(1-Elteq!$F$6)","v":17.744489623580915}]
["ANAMET-S",7149351,"NPT 1.1/4\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,27.685119936267604,{"$f":"F1403*(1-Elteq!$F$6)","v":27.685119936267604}]
["ANAMET-S",7149352,"NPT 1.1/4\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,28.511957410874253,{"$f":"F1404*(1-Elteq!$F$6)","v":28.511957410874253}]
["ANAMET-S",7149401,"NPT 1.1/2\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,37.309879753037144,{"$f":"F1405*(1-Elteq!$F$6)","v":37.309879753037144}]
["ANAMET-S",7149402,"NPT 1.1/2\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,38.341104019119598,{"$f":"F1406*(1-Elteq!$F$6)","v":38.341104019119598}]
["ANAMET-S",7149501,"NPT 2\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,56.011271173072949,{"$f":"F1407*(1-Elteq!$F$6)","v":56.011271173072949}]
["ANAMET-S",7149502,"NPT 2\"","Compact fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,57.47913994821733,{"$f":"F1408*(1-Elteq!$F$6)","v":57.47913994821733}]
["ANAMET-S",8150112,"3/8\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",50,0.73393438757219487,{"$f":"F1409*(1-Elteq!$F$6)","v":0.73393438757219487}]
["ANAMET-S",8150162,"1/2\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",50,0.78038593108942222,{"$f":"F1410*(1-Elteq!$F$6)","v":0.78038593108942222}]
["ANAMET-S",8150212,"3/4\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",25,0.83612778331009541,{"$f":"F1411*(1-Elteq!$F$6)","v":0.83612778331009541}]
["ANAMET-S",8150292,"1\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",25,0.89186963553076837,{"$f":"F1412*(1-Elteq!$F$6)","v":0.89186963553076837}]
["ANAMET-S",8150362,"1.1/4\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",10,1.3470947619995981,{"$f":"F1413*(1-Elteq!$F$6)","v":1.3470947619995981}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8150422,"1 1/2\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",10,1.7930295797649822,{"$f":"F1414*(1-Elteq!$F$6)","v":1.7930295797649822}]
["ANAMET-S",8150482,"2\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",10,2.8149635371439876,{"$f":"F1415*(1-Elteq!$F$6)","v":2.8149635371439876}]
["ANAMET-S",8130150,"M16 x 1,5","Swivel fittings for Sealtite, Straight swivel with male thread, IP 67",10,7.1814086277633749,{"$f":"F1416*(1-Elteq!$F$6)","v":7.1814086277633749}]
["ANAMET-S",8130160,"M16 x 1,5","Swivel fittings for Sealtite, Straight swivel with male thread, IP 67",10,6.5589579446325255,{"$f":"F1417*(1-Elteq!$F$6)","v":6.5589579446325255}]
["ANAMET-S",8130200,"M20 x 1,5","Swivel fittings for Sealtite, Straight swivel with male thread, IP 67",10,7.4508275801632937,{"$f":"F1418*(1-Elteq!$F$6)","v":7.4508275801632937}]
["ANAMET-S",8130250,"M25 x 1,5","Swivel fittings for Sealtite, Straight swivel with male thread, IP 67",5,9.8105659908384535,{"$f":"F1419*(1-Elteq!$F$6)","v":9.8105659908384535}]
["ANAMET-S",8130320,"M32 x 1,5","Swivel fittings for Sealtite, Straight swivel with male thread, IP 67",5,16.323072391953751,{"$f":"F1420*(1-Elteq!$F$6)","v":16.323072391953751}]
["ANAMET-S",8130400,"M40 x 1,5","Swivel fittings for Sealtite, Straight swivel with male thread, IP 67",2,18.850036359290925,{"$f":"F1421*(1-Elteq!$F$6)","v":18.850036359290925}]
["ANAMET-S",8130500,"M50 x 1,5","Swivel fittings for Sealtite, Straight swivel with male thread, IP 67",2,33.212853614817682,{"$f":"F1422*(1-Elteq!$F$6)","v":33.212853614817682}]
["ANAMET-S",8130630,"M63 x 1,5","Swivel fittings for Sealtite, Straight swivel with male thread, IP 67",2,49.498764771957646,{"$f":"F1423*(1-Elteq!$F$6)","v":49.498764771957646}]
["ANAMET-S",8134160,"M16 x 1,5","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",10,13.294431754630518,{"$f":"F1424*(1-Elteq!$F$6)","v":13.294431754630518}]
["ANAMET-S",8134200,"M20 x 1,5","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",10,17.317135423222421,{"$f":"F1425*(1-Elteq!$F$6)","v":17.317135423222421}]
["ANAMET-S",8134250,"M25 x 1,5","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",5,24.730801768571933,{"$f":"F1426*(1-Elteq!$F$6)","v":24.730801768571933}]
["ANAMET-S",8134320,"M32 x 1,5","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",5,39.418779828719273,{"$f":"F1427*(1-Elteq!$F$6)","v":39.418779828719273}]
["ANAMET-S",8139150,"M16 x 1,5","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",10,13.062174037044379,{"$f":"F1428*(1-Elteq!$F$6)","v":13.062174037044379}]
["ANAMET-S",8139160,"M16 x 1,5","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",10,11.519982792272426,{"$f":"F1429*(1-Elteq!$F$6)","v":11.519982792272426}]
["ANAMET-S",8139200,"M20 x 1,5","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",10,14.920235777733479,{"$f":"F1430*(1-Elteq!$F$6)","v":14.920235777733479}]
["ANAMET-S",8139250,"M25 x 1,5","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",5,23.959706146185955,{"$f":"F1431*(1-Elteq!$F$6)","v":23.959706146185955}]
["ANAMET-S",8139320,"M32 x 1,5","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",5,38.573361736705735,{"$f":"F1432*(1-Elteq!$F$6)","v":38.573361736705735}]
["ANAMET-S",8194120,"NPT 1/2\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",10,13.294431754630518,{"$f":"F1433*(1-Elteq!$F$6)","v":13.294431754630518}]
["ANAMET-S",8194160,"NPT 1/2\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",10,17.317135423222421,{"$f":"F1434*(1-Elteq!$F$6)","v":17.317135423222421}]
["ANAMET-S",8194200,"NPT 3/4\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",5,24.730801768571933,{"$f":"F1435*(1-Elteq!$F$6)","v":24.730801768571933}]
["ANAMET-S",8194260,"NPT 1\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",5,39.418779828719273,{"$f":"F1436*(1-Elteq!$F$6)","v":39.418779828719273}]
["ANAMET-S",8199120,"NPT 1/2\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",10,13.294431754630518,{"$f":"F1437*(1-Elteq!$F$6)","v":13.294431754630518}]
["ANAMET-S",8199160,"NPT 1/2\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",10,17.317135423222421,{"$f":"F1438*(1-Elteq!$F$6)","v":17.317135423222421}]
["ANAMET-S",8199200,"NPT 3/4\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",5,24.730801768571933,{"$f":"F1439*(1-Elteq!$F$6)","v":24.730801768571933}]
["ANAMET-S",8199260,"NPT 1\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",5,39.418779828719273,{"$f":"F1440*(1-Elteq!$F$6)","v":39.418779828719273}]
["ANAMET-S",8120112,"M12 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,4.5057997211710692,{"$f":"F1441*(1-Elteq!$F$6)","v":4.5057997211710692}]
["ANAMET-S",8120121,"M12 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,4.8588314519019988,{"$f":"F1442*(1-Elteq!$F$6)","v":4.8588314519019988}]
["ANAMET-S",8120122,"M12 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,4.3664450906193863,{"$f":"F1443*(1-Elteq!$F$6)","v":4.3664450906193863}]
["ANAMET-S",8120132,"M16 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,4.3664450906193863,{"$f":"F1444*(1-Elteq!$F$6)","v":4.3664450906193863}]
["ANAMET-S",8120141,"M20 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,5.6949592352120932,{"$f":"F1445*(1-Elteq!$F$6)","v":5.6949592352120932}]
["ANAMET-S",8120142,"M20 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,4.5057997211710692,{"$f":"F1446*(1-Elteq!$F$6)","v":4.5057997211710692}]
["ANAMET-S",8120151,"M16 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,4.4128966341366143,{"$f":"F1447*(1-Elteq!$F$6)","v":4.4128966341366143}]
["ANAMET-S",8120152,"M16 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,4.1527679904401404,{"$f":"F1448*(1-Elteq!$F$6)","v":4.1527679904401404}]
["ANAMET-S",8120161,"M16 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,3.8183168771161027,{"$f":"F1449*(1-Elteq!$F$6)","v":3.8183168771161027}]
["ANAMET-S",8120171,"M20 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,4.1063164469229125,{"$f":"F1450*(1-Elteq!$F$6)","v":4.1063164469229125}]
["ANAMET-S",8120201,"M20 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,4.1063164469229125,{"$f":"F1451*(1-Elteq!$F$6)","v":4.1063164469229125}]
["ANAMET-S",8120251,"M25 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",5,6.0572812746464679,{"$f":"F1452*(1-Elteq!$F$6)","v":6.0572812746464679}]
["ANAMET-S",8120321,"M32 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",5,9.7455338299143328,{"$f":"F1453*(1-Elteq!$F$6)","v":9.7455338299143328}]
["ANAMET-S",8120401,"M40 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",2,17.846683019318814,{"$f":"F1454*(1-Elteq!$F$6)","v":17.846683019318814}]
["ANAMET-S",8120501,"M50 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",2,23.95041583748251,{"$f":"F1455*(1-Elteq!$F$6)","v":23.95041583748251}]
["ANAMET-S",8120631,"M63 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",2,36.724590304720074,{"$f":"F1456*(1-Elteq!$F$6)","v":36.724590304720074}]
["ANAMET-S",8120751,"M75 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",1,194.24177437163863,{"$f":"F1457*(1-Elteq!$F$6)","v":194.24177437163863}]
["ANAMET-S",8123151,"M16 x 1,5","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",10,5.7692817048396581,{"$f":"F1458*(1-Elteq!$F$6)","v":5.7692817048396581}]
["ANAMET-S",8123161,"M16 x 1,5","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",10,4.5801221907986331,{"$f":"F1459*(1-Elteq!$F$6)","v":4.5801221907986331}]
["ANAMET-S",8123201,"M20 x 1,5","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",10,4.9238636128261177,{"$f":"F1460*(1-Elteq!$F$6)","v":4.9238636128261177}]
["ANAMET-S",8123251,"M25 x 1,5","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",5,7.2650214060943847,{"$f":"F1461*(1-Elteq!$F$6)","v":7.2650214060943847}]
["ANAMET-S",8123321,"M32 x 1,5","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",5,10.39585543915552,{"$f":"F1462*(1-Elteq!$F$6)","v":10.39585543915552}]
["ANAMET-S",8123401,"M40 x 1,5","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",2,23.838932133041162,{"$f":"F1463*(1-Elteq!$F$6)","v":23.838932133041162}]
["ANAMET-S",8123501,"M50 x 1,5","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",2,31.438404652459589,{"$f":"F1464*(1-Elteq!$F$6)","v":31.438404652459589}]
["ANAMET-S",8123631,"M63 x 1,5","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",2,47.324832535351391,{"$f":"F1465*(1-Elteq!$F$6)","v":47.324832535351391}]
["ANAMET-S",8124141,"M20 x 1,5","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,9.281018394742059,{"$f":"F1466*(1-Elteq!$F$6)","v":9.281018394742059}]
["ANAMET-S",8124151,"M16 x 1,5","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,7.7574077673769963,{"$f":"F1467*(1-Elteq!$F$6)","v":7.7574077673769963}]
["ANAMET-S",8124161,"M16 x 1,5","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,6.958441218880683,{"$f":"F1468*(1-Elteq!$F$6)","v":6.958441218880683}]
["ANAMET-S",8124171,"M20 x 1,5","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,8.0918588807010359,{"$f":"F1469*(1-Elteq!$F$6)","v":8.0918588807010359}]
["ANAMET-S",8124201,"M20 x 1,5","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,8.0918588807010359,{"$f":"F1470*(1-Elteq!$F$6)","v":8.0918588807010359}]
["ANAMET-S",8124251,"M25 x 1,5","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",5,10.609532539334765,{"$f":"F1471*(1-Elteq!$F$6)","v":10.609532539334765}]
["ANAMET-S",8124321,"M32 x 1,5","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",5,21.897257614021054,{"$f":"F1472*(1-Elteq!$F$6)","v":21.897257614021054}]
["ANAMET-S",8124401,"M40 x 1,5","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",2,28.744215128460393,{"$f":"F1473*(1-Elteq!$F$6)","v":28.744215128460393}]
["ANAMET-S",8124501,"M50 x 1,5","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",2,41.65774422624964,{"$f":"F1474*(1-Elteq!$F$6)","v":41.65774422624964}]
["ANAMET-S",8124631,"M63 x 1,5","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",2,60.238361633140649,{"$f":"F1475*(1-Elteq!$F$6)","v":60.238361633140649}]
["ANAMET-S",8129141,"M20 x 1,5","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,9.281018394742059,{"$f":"F1476*(1-Elteq!$F$6)","v":9.281018394742059}]
["ANAMET-S",8129151,"M16 x 1,5","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,8.1476007329217079,{"$f":"F1477*(1-Elteq!$F$6)","v":8.1476007329217079}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8129161,"M16 x 1,5","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,6.958441218880683,{"$f":"F1478*(1-Elteq!$F$6)","v":6.958441218880683}]
["ANAMET-S",8129171,"M20 x 1,5","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,8.0918588807010359,{"$f":"F1479*(1-Elteq!$F$6)","v":8.0918588807010359}]
["ANAMET-S",8129201,"M20 x 1,5","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,8.0918588807010359,{"$f":"F1480*(1-Elteq!$F$6)","v":8.0918588807010359}]
["ANAMET-S",8129251,"M25 x 1,5","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",5,10.609532539334765,{"$f":"F1481*(1-Elteq!$F$6)","v":10.609532539334765}]
["ANAMET-S",8129321,"M32 x 1,5","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",5,21.897257614021054,{"$f":"F1482*(1-Elteq!$F$6)","v":21.897257614021054}]
["ANAMET-S",8129401,"M40 x 1,5","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,28.744215128460393,{"$f":"F1483*(1-Elteq!$F$6)","v":28.744215128460393}]
["ANAMET-S",8129501,"M50 x 1,5","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,41.65774422624964,{"$f":"F1484*(1-Elteq!$F$6)","v":41.65774422624964}]
["ANAMET-S",8129631,"M63 x 1,5","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,64.632677649870359,{"$f":"F1485*(1-Elteq!$F$6)","v":64.632677649870359}]
["ANAMET-S",7852340,"1/2”","Standard fittings for Sealtite, Multiple seals for cable hose fittings",100,0.863998709420432,{"$f":"F1486*(1-Elteq!$F$6)","v":0.863998709420432}]
["ANAMET-S",7852350,"1/2”","Standard fittings for Sealtite, Multiple seals for cable hose fittings",100,0.863998709420432,{"$f":"F1487*(1-Elteq!$F$6)","v":0.863998709420432}]
["ANAMET-S",7852430,"1/2”","Standard fittings for Sealtite, Multiple seals for cable hose fittings",100,0.863998709420432,{"$f":"F1488*(1-Elteq!$F$6)","v":0.863998709420432}]
["ANAMET-S",7852440,"1/2”","Standard fittings for Sealtite, Multiple seals for cable hose fittings",100,0.863998709420432,{"$f":"F1489*(1-Elteq!$F$6)","v":0.863998709420432}]
["ANAMET-S",7853270,"3/4”","Standard fittings for Sealtite, Multiple seals for cable hose fittings",100,0.97548241386177792,{"$f":"F1490*(1-Elteq!$F$6)","v":0.97548241386177792}]
["ANAMET-S",7853366,"3/4”","Standard fittings for Sealtite, Multiple seals for cable hose fittings",100,0.97548241386177792,{"$f":"F1491*(1-Elteq!$F$6)","v":0.97548241386177792}]
["ANAMET-S",7853380,"3/4”","Standard fittings for Sealtite, Multiple seals for cable hose fittings",100,0.97548241386177792,{"$f":"F1492*(1-Elteq!$F$6)","v":0.97548241386177792}]
["ANAMET-S",7854375,"1”","Standard fittings for Sealtite, Multiple seals for cable hose fittings",100,1.5329009360685082,{"$f":"F1493*(1-Elteq!$F$6)","v":1.5329009360685082}]
["ANAMET-S",7854480,"1”","Standard fittings for Sealtite, Multiple seals for cable hose fittings",100,1.5329009360685082,{"$f":"F1494*(1-Elteq!$F$6)","v":1.5329009360685082}]
["ANAMET-S",7854650,"1”","Standard fittings for Sealtite, Multiple seals for cable hose fittings",100,1.5329009360685082,{"$f":"F1495*(1-Elteq!$F$6)","v":1.5329009360685082}]
["ANAMET-S",7854660,"1”","Standard fittings for Sealtite, Multiple seals for cable hose fittings",100,1.5329009360685082,{"$f":"F1496*(1-Elteq!$F$6)","v":1.5329009360685082}]
["ANAMET-S",8126152,"M16 x 1,5","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",10,16.090814674367611,{"$f":"F1497*(1-Elteq!$F$6)","v":16.090814674367611}]
["ANAMET-S",8126161,"M16 x 1,5","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",10,16.090814674367611,{"$f":"F1498*(1-Elteq!$F$6)","v":16.090814674367611}]
["ANAMET-S",8126171,"M16 x 1,5","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",10,16.090814674367611,{"$f":"F1499*(1-Elteq!$F$6)","v":16.090814674367611}]
["ANAMET-S",8126201,"M20 x 1,5","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",10,18.673520493925462,{"$f":"F1500*(1-Elteq!$F$6)","v":18.673520493925462}]
["ANAMET-S",8126221,"M25 x 1,5","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",10,23.764609663413598,{"$f":"F1501*(1-Elteq!$F$6)","v":23.764609663413598}]
["ANAMET-S",8126281,"M32 x 1,5","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",5,33.668078741286507,{"$f":"F1502*(1-Elteq!$F$6)","v":33.668078741286507}]
["ANAMET-S",8126351,"M40 x 1,5","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",5,52.285857382991296,{"$f":"F1503*(1-Elteq!$F$6)","v":52.285857382991296}]
["ANAMET-S",8127152,"M16 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",10,10.024243091017699,{"$f":"F1504*(1-Elteq!$F$6)","v":10.024243091017699}]
["ANAMET-S",8127161,"M16 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",10,10.024243091017699,{"$f":"F1505*(1-Elteq!$F$6)","v":10.024243091017699}]
["ANAMET-S",8127162,"M16 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",10,11.984498227444702,{"$f":"F1506*(1-Elteq!$F$6)","v":11.984498227444702}]
["ANAMET-S",8127171,"M20 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",10,10.024243091017699,{"$f":"F1507*(1-Elteq!$F$6)","v":10.024243091017699}]
["ANAMET-S",8127201,"M20 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",10,11.585014953196543,{"$f":"F1508*(1-Elteq!$F$6)","v":11.585014953196543}]
["ANAMET-S",8127202,"M20 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",10,13.731076263692454,{"$f":"F1509*(1-Elteq!$F$6)","v":13.731076263692454}]
["ANAMET-S",8127221,"M25 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",10,14.632236207926669,{"$f":"F1510*(1-Elteq!$F$6)","v":14.632236207926669}]
["ANAMET-S",8127252,"M25 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",5,19.305261485759761,{"$f":"F1511*(1-Elteq!$F$6)","v":19.305261485759761}]
["ANAMET-S",8127281,"M32 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",5,23.123578362875861,{"$f":"F1512*(1-Elteq!$F$6)","v":23.123578362875861}]
["ANAMET-S",8127322,"M32 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",5,49.23863612826117,{"$f":"F1513*(1-Elteq!$F$6)","v":49.23863612826117}]
["ANAMET-S",8127351,"M40 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",5,34.699303007368961,{"$f":"F1514*(1-Elteq!$F$6)","v":34.699303007368961}]
["ANAMET-S",8127402,"M40 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",2,64.929967528380629,{"$f":"F1515*(1-Elteq!$F$6)","v":64.929967528380629}]
["ANAMET-S",8127502,"M50 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",2,93.367602469627315,{"$f":"F1516*(1-Elteq!$F$6)","v":93.367602469627315}]
["ANAMET-S",8127632,"M63 x 1,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",2,140.5623706831305,{"$f":"F1517*(1-Elteq!$F$6)","v":140.5623706831305}]
["ANAMET-S",8100071,"PG 7","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,4.8588314519019988,{"$f":"F1518*(1-Elteq!$F$6)","v":4.8588314519019988}]
["ANAMET-S",8100072,"PG 7","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,4.3664450906193863,{"$f":"F1519*(1-Elteq!$F$6)","v":4.3664450906193863}]
["ANAMET-S",8100091,"PG 9","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,5.2397341087432645,{"$f":"F1520*(1-Elteq!$F$6)","v":5.2397341087432645}]
["ANAMET-S",8100092,"PG 9","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,4.3664450906193863,{"$f":"F1521*(1-Elteq!$F$6)","v":4.3664450906193863}]
["ANAMET-S",8100101,"PG 9","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,3.9669618163712301,{"$f":"F1522*(1-Elteq!$F$6)","v":3.9669618163712301}]
["ANAMET-S",8100111,"PG 11","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,4.0784455208125756,{"$f":"F1523*(1-Elteq!$F$6)","v":4.0784455208125756}]
["ANAMET-S",8100121,"PG 11","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,5.2025728739294816,{"$f":"F1524*(1-Elteq!$F$6)","v":5.2025728739294816}]
["ANAMET-S",8100131,"PG 13,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,4.0784455208125756,{"$f":"F1525*(1-Elteq!$F$6)","v":4.0784455208125756}]
["ANAMET-S",8100141,"PG 13,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,5.3233468870742744,{"$f":"F1526*(1-Elteq!$F$6)","v":5.3233468870742744}]
["ANAMET-S",8100161,"PG 16","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,4.756638056164098,{"$f":"F1527*(1-Elteq!$F$6)","v":4.756638056164098}]
["ANAMET-S",8100211,"PG 21","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",5,6.2988293009360516,{"$f":"F1528*(1-Elteq!$F$6)","v":6.2988293009360516}]
["ANAMET-S",8100291,"PG 29","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",5,10.888241800438133,{"$f":"F1529*(1-Elteq!$F$6)","v":10.888241800438133}]
["ANAMET-S",8100361,"PG 36","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",2,17.846683019318814,{"$f":"F1530*(1-Elteq!$F$6)","v":17.846683019318814}]
["ANAMET-S",8100421,"PG 42","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",2,23.95041583748251,{"$f":"F1531*(1-Elteq!$F$6)","v":23.95041583748251}]
["ANAMET-S",8100481,"PG 48","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",2,36.724590304720074,{"$f":"F1532*(1-Elteq!$F$6)","v":36.724590304720074}]
["ANAMET-S",8103111,"PG 11","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",10,4.803089599681325,{"$f":"F1533*(1-Elteq!$F$6)","v":4.803089599681325}]
["ANAMET-S",8103121,"PG 11","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",10,5.9922491137223508,{"$f":"F1534*(1-Elteq!$F$6)","v":5.9922491137223508}]
["ANAMET-S",8103131,"PG 13,5","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",10,4.803089599681325,{"$f":"F1535*(1-Elteq!$F$6)","v":4.803089599681325}]
["ANAMET-S",8103141,"PG 13,5","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",10,5.9922491137223508,{"$f":"F1536*(1-Elteq!$F$6)","v":5.9922491137223508}]
["ANAMET-S",8103161,"PG 16","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",10,5.1189600955984718,{"$f":"F1537*(1-Elteq!$F$6)","v":5.1189600955984718}]
["ANAMET-S",8103211,"PG 21","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",5,7.5530209759011955,{"$f":"F1538*(1-Elteq!$F$6)","v":7.5530209759011955}]
["ANAMET-S",8103291,"PG 29","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",5,10.804629022107122,{"$f":"F1539*(1-Elteq!$F$6)","v":10.804629022107122}]
["ANAMET-S",8103361,"PG 36","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",2,23.838932133041162,{"$f":"F1540*(1-Elteq!$F$6)","v":23.838932133041162}]
["ANAMET-S",8103421,"PG 42","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",2,34.281239115713909,{"$f":"F1541*(1-Elteq!$F$6)","v":34.281239115713909}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8103481,"PG 48","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",2,47.324832535351391,{"$f":"F1542*(1-Elteq!$F$6)","v":47.324832535351391}]
["ANAMET-S",8104111,"PG 11","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,6.958441218880683,{"$f":"F1543*(1-Elteq!$F$6)","v":6.958441218880683}]
["ANAMET-S",8104121,"PG 11","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,8.4727615375422989,{"$f":"F1544*(1-Elteq!$F$6)","v":8.4727615375422989}]
["ANAMET-S",8104131,"PG 13,5","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,7.2278601712806028,{"$f":"F1545*(1-Elteq!$F$6)","v":7.2278601712806028}]
["ANAMET-S",8104141,"PG 13,5","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,8.4727615375422989,{"$f":"F1546*(1-Elteq!$F$6)","v":8.4727615375422989}]
["ANAMET-S",8104161,"PG 16","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,8.4077293766181818,{"$f":"F1547*(1-Elteq!$F$6)","v":8.4077293766181818}]
["ANAMET-S",8104211,"PG 21","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",5,11.027596430989814,{"$f":"F1548*(1-Elteq!$F$6)","v":11.027596430989814}]
["ANAMET-S",8104291,"PG 29","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",5,22.770546632144935,{"$f":"F1549*(1-Elteq!$F$6)","v":22.770546632144935}]
["ANAMET-S",8104361,"PG 36","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",2,30.862405512845964,{"$f":"F1550*(1-Elteq!$F$6)","v":30.862405512845964}]
["ANAMET-S",8104421,"PG 42","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",2,44.742126715793546,{"$f":"F1551*(1-Elteq!$F$6)","v":44.742126715793546}]
["ANAMET-S",8104481,"PG 48","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",2,64.697709810794493,{"$f":"F1552*(1-Elteq!$F$6)","v":64.697709810794493}]
["ANAMET-S",8106091,"PG 9","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",10,17.279974188408641,{"$f":"F1553*(1-Elteq!$F$6)","v":17.279974188408641}]
["ANAMET-S",8106111,"PG 11","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",10,16.090814674367611,{"$f":"F1554*(1-Elteq!$F$6)","v":16.090814674367611}]
["ANAMET-S",8106121,"PG 9","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",10,16.090814674367611,{"$f":"F1555*(1-Elteq!$F$6)","v":16.090814674367611}]
["ANAMET-S",8106151,"PG 13,5","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",10,16.090814674367611,{"$f":"F1556*(1-Elteq!$F$6)","v":16.090814674367611}]
["ANAMET-S",8106161,"PG 16","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",10,18.673520493925462,{"$f":"F1557*(1-Elteq!$F$6)","v":18.673520493925462}]
["ANAMET-S",8106211,"PG 21","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",5,33.668078741286507,{"$f":"F1558*(1-Elteq!$F$6)","v":33.668078741286507}]
["ANAMET-S",8106291,"PG 29","Standard fittings for Sealtite, Straight EMC cablehose male thread IP 68",5,52.285857382991296,{"$f":"F1559*(1-Elteq!$F$6)","v":52.285857382991296}]
["ANAMET-S",8107091,"PG 9","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",10,11.399208779127633,{"$f":"F1560*(1-Elteq!$F$6)","v":11.399208779127633}]
["ANAMET-S",8107111,"PG 11","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",10,10.024243091017699,{"$f":"F1561*(1-Elteq!$F$6)","v":10.024243091017699}]
["ANAMET-S",8107121,"PG 9","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",10,10.024243091017699,{"$f":"F1562*(1-Elteq!$F$6)","v":10.024243091017699}]
["ANAMET-S",8107151,"PG 13,5","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",10,11.585014953196543,{"$f":"F1563*(1-Elteq!$F$6)","v":11.585014953196543}]
["ANAMET-S",8107161,"PG 16","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",10,14.632236207926669,{"$f":"F1564*(1-Elteq!$F$6)","v":14.632236207926669}]
["ANAMET-S",8107211,"PG 21","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",5,23.123578362875861,{"$f":"F1565*(1-Elteq!$F$6)","v":23.123578362875861}]
["ANAMET-S",8107291,"PG 29","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",5,34.699303007368961,{"$f":"F1566*(1-Elteq!$F$6)","v":34.699303007368961}]
["ANAMET-S",8109111,"PG 11","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,6.958441218880683,{"$f":"F1567*(1-Elteq!$F$6)","v":6.958441218880683}]
["ANAMET-S",8109121,"PG 11","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,8.4727615375422989,{"$f":"F1568*(1-Elteq!$F$6)","v":8.4727615375422989}]
["ANAMET-S",8109131,"PG 13,5","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,7.2278601712806028,{"$f":"F1569*(1-Elteq!$F$6)","v":7.2278601712806028}]
["ANAMET-S",8109141,"PG 13,5","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,8.4727615375422989,{"$f":"F1570*(1-Elteq!$F$6)","v":8.4727615375422989}]
["ANAMET-S",8109161,"PG 16","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,8.4077293766181818,{"$f":"F1571*(1-Elteq!$F$6)","v":8.4077293766181818}]
["ANAMET-S",8109211,"PG 21","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",5,11.027596430989814,{"$f":"F1572*(1-Elteq!$F$6)","v":11.027596430989814}]
["ANAMET-S",8109291,"PG 29","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",5,22.770546632144935,{"$f":"F1573*(1-Elteq!$F$6)","v":22.770546632144935}]
["ANAMET-S",8109361,"PG 36","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,30.862405512845964,{"$f":"F1574*(1-Elteq!$F$6)","v":30.862405512845964}]
["ANAMET-S",8109421,"PG 42","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,44.742126715793546,{"$f":"F1575*(1-Elteq!$F$6)","v":44.742126715793546}]
["ANAMET-S",8109481,"PG 48","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,64.697709810794493,{"$f":"F1576*(1-Elteq!$F$6)","v":64.697709810794493}]
["ANAMET-S",8140111,"NPT 1/2\"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,5.4162499741087293,{"$f":"F1577*(1-Elteq!$F$6)","v":5.4162499741087293}]
["ANAMET-S",8140121,"NPT 1/2\"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,4.3943160167297233,{"$f":"F1578*(1-Elteq!$F$6)","v":4.3943160167297233}]
["ANAMET-S",8140161,"NPT 1/2\"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,4.6265737343158611,{"$f":"F1579*(1-Elteq!$F$6)","v":4.6265737343158611}]
["ANAMET-S",8140201,"NPT 3/4\"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",5,5.927216952798231,{"$f":"F1580*(1-Elteq!$F$6)","v":5.927216952798231}]
["ANAMET-S",8140261,"NPT 1 \"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",5,9.8663078430591238,{"$f":"F1581*(1-Elteq!$F$6)","v":9.8663078430591238}]
["ANAMET-S",8140351,"NPT 1.1/4 \"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",2,18.497004628559999,{"$f":"F1582*(1-Elteq!$F$6)","v":18.497004628559999}]
["ANAMET-S",8140401,"NPT 1.1/2\"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",2,26.393767026488675,{"$f":"F1583*(1-Elteq!$F$6)","v":26.393767026488675}]
["ANAMET-S",8140501,"NPT 2\"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",2,41.490518669587622,{"$f":"F1584*(1-Elteq!$F$6)","v":41.490518669587622}]
["ANAMET-S",8144111,"NPT 1/2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,8.4263099940250736,{"$f":"F1585*(1-Elteq!$F$6)","v":8.4263099940250736}]
["ANAMET-S",8144121,"NPT 1/2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,7.2371504799840478,{"$f":"F1586*(1-Elteq!$F$6)","v":7.2371504799840478}]
["ANAMET-S",8144161,"NPT 1/2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,7.7388271499701045,{"$f":"F1587*(1-Elteq!$F$6)","v":7.7388271499701045}]
["ANAMET-S",8144201,"NPT 3/4\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",5,10.470177908783082,{"$f":"F1588*(1-Elteq!$F$6)","v":10.470177908783082}]
["ANAMET-S",8144261,"NPT 1 \"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",5,19.295971177056312,{"$f":"F1589*(1-Elteq!$F$6)","v":19.295971177056312}]
["ANAMET-S",8144351,"NPT 1.1/4 \"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",2,31.271179095797564,{"$f":"F1590*(1-Elteq!$F$6)","v":31.271179095797564}]
["ANAMET-S",8144401,"NPT 1.1/2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",2,40.635810268870635,{"$f":"F1591*(1-Elteq!$F$6)","v":40.635810268870635}]
["ANAMET-S",8144501,"NPT 2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",2,63.397066592312115,{"$f":"F1592*(1-Elteq!$F$6)","v":63.397066592312115}]
["ANAMET-S",8149111,"NPT 1/2\"","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,8.4263099940250736,{"$f":"F1593*(1-Elteq!$F$6)","v":8.4263099940250736}]
["ANAMET-S",8149121,"NPT 1/2\"","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,7.2371504799840478,{"$f":"F1594*(1-Elteq!$F$6)","v":7.2371504799840478}]
["ANAMET-S",8149161,"NPT 1/2\"","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,8.1568910416251512,{"$f":"F1595*(1-Elteq!$F$6)","v":8.1568910416251512}]
["ANAMET-S",8149201,"NPT 3/4\"","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",5,10.888241800438133,{"$f":"F1596*(1-Elteq!$F$6)","v":10.888241800438133}]
["ANAMET-S",8149261,"NPT 1 \"","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",5,19.295971177056312,{"$f":"F1597*(1-Elteq!$F$6)","v":19.295971177056312}]
["ANAMET-S",8149351,"NPT 1.1/4 \"","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,31.271179095797564,{"$f":"F1598*(1-Elteq!$F$6)","v":31.271179095797564}]
["ANAMET-S",8149401,"NPT 1.1/2\"","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,40.635810268870635,{"$f":"F1599*(1-Elteq!$F$6)","v":40.635810268870635}]
["ANAMET-S",8149501,"NPT 2\"","Standard fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,63.397066592312115,{"$f":"F1600*(1-Elteq!$F$6)","v":63.397066592312115}]
["ANAMET-S",8143111,"NPT 1/2\"","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",10,5.9922491137223508,{"$f":"F1601*(1-Elteq!$F$6)","v":5.9922491137223508}]
["ANAMET-S",8143121,"NPT 1/2\"","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",10,4.803089599681325,{"$f":"F1602*(1-Elteq!$F$6)","v":4.803089599681325}]
["ANAMET-S",8143161,"NPT 1/2\"","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",10,5.1561213304122546,{"$f":"F1603*(1-Elteq!$F$6)","v":5.1561213304122546}]
["ANAMET-S",8143201,"NPT 3/4\"","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",5,7.6180531368253126,{"$f":"F1604*(1-Elteq!$F$6)","v":7.6180531368253126}]
["ANAMET-S",8143261,"NPT 1 \"","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",5,10.888241800438133,{"$f":"F1605*(1-Elteq!$F$6)","v":10.888241800438133}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8143351,"NPT 1.1/4 \"","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",2,24.034028615813519,{"$f":"F1606*(1-Elteq!$F$6)","v":24.034028615813519}]
["ANAMET-S",8143401,"NPT 1.1/2\"","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",2,35.135947516430896,{"$f":"F1607*(1-Elteq!$F$6)","v":35.135947516430896}]
["ANAMET-S",8143501,"NPT 2\"","Standard fittings for Sealtite, Straight fixed with female thread, IP 67",2,53.42856535351509,{"$f":"F1608*(1-Elteq!$F$6)","v":53.42856535351509}]
["ANAMET-S",8147091,"NPT 3/8\"","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",10,11.213402605058723,{"$f":"F1609*(1-Elteq!$F$6)","v":11.213402605058723}]
["ANAMET-S",8147101,"NPT 3/8\"","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",10,10.024243091017699,{"$f":"F1610*(1-Elteq!$F$6)","v":10.024243091017699}]
["ANAMET-S",8147121,"NPT 1/2\"","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",10,10.024243091017699,{"$f":"F1611*(1-Elteq!$F$6)","v":10.024243091017699}]
["ANAMET-S",8147151,"NPT 1/2\"","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",10,14.632236207926669,{"$f":"F1612*(1-Elteq!$F$6)","v":14.632236207926669}]
["ANAMET-S",8147211,"NPT 3/4\"","Standard fittings for Sealtite, Straight cablehose male thread, IP 68",5,23.123578362875861,{"$f":"F1613*(1-Elteq!$F$6)","v":23.123578362875861}]
["ANAMET-S",8150060,"1/4\"","Standard fittings for Sealtite, Ferrule, nickel plated brass",10,2.0252872973511198,{"$f":"F1614*(1-Elteq!$F$6)","v":2.0252872973511198}]
["ANAMET-S",8150100,"5/16\"","Standard fittings for Sealtite, Ferrule, nickel plated brass",10,2.0252872973511198,{"$f":"F1615*(1-Elteq!$F$6)","v":2.0252872973511198}]
["ANAMET-S",8150110,"3/8\"","Standard fittings for Sealtite, Ferrule, galvanised steel",10,0.91974056164110485,{"$f":"F1616*(1-Elteq!$F$6)","v":0.91974056164110485}]
["ANAMET-S",8150113,"3/8\"","Standard fittings for Sealtite, Ferrule, nickel plated brass",10,2.303996558454485,{"$f":"F1617*(1-Elteq!$F$6)","v":2.303996558454485}]
["ANAMET-S",8150160,"1/2\"","Standard fittings for Sealtite, Ferrule, galvanised steel",10,0.97548241386177792,{"$f":"F1618*(1-Elteq!$F$6)","v":0.97548241386177792}]
["ANAMET-S",8150163,"1/2\"","Standard fittings for Sealtite, Ferrule, nickel plated brass",10,2.7778023023302061,{"$f":"F1619*(1-Elteq!$F$6)","v":2.7778023023302061}]
["ANAMET-S",8150210,"3/4\"","Standard fittings for Sealtite, Ferrule, galvanised steel",5,1.0405145747858966,{"$f":"F1620*(1-Elteq!$F$6)","v":1.0405145747858966}]
["ANAMET-S",8150213,"3/4\"","Standard fittings for Sealtite, Ferrule, nickel plated brass",5,3.3073498984265992,{"$f":"F1621*(1-Elteq!$F$6)","v":3.3073498984265992}]
["ANAMET-S",8150290,"1\"","Standard fittings for Sealtite, Ferrule, galvanised steel",2,1.1148370444134605,{"$f":"F1622*(1-Elteq!$F$6)","v":1.1148370444134605}]
["ANAMET-S",8150293,"1\"","Standard fittings for Sealtite, Ferrule, nickel plated brass",5,4.4314772515435052,{"$f":"F1623*(1-Elteq!$F$6)","v":4.4314772515435052}]
["ANAMET-S",8150363,"1 1/4\"","Standard fittings for Sealtite, Ferrule, nickel plated brass",2,5.815733248356886,{"$f":"F1624*(1-Elteq!$F$6)","v":5.815733248356886}]
["ANAMET-S",8150423,"1 1/2\"","Standard fittings for Sealtite, Ferrule, nickel plated brass",2,8.0268267197769152,{"$f":"F1625*(1-Elteq!$F$6)","v":8.0268267197769152}]
["ANAMET-S",8150483,"2\"","Standard fittings for Sealtite, Ferrule, nickel plated brass",2,12.049530388368819,{"$f":"F1626*(1-Elteq!$F$6)","v":12.049530388368819}]
["ANAMET-S",8154160,"M 16","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,0.34374142202748365,{"$f":"F1627*(1-Elteq!$F$6)","v":0.34374142202748365}]
["ANAMET-S",8154200,"M 20","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,0.37161234813782018,{"$f":"F1628*(1-Elteq!$F$6)","v":0.37161234813782018}]
["ANAMET-S",8154250,"M 25","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,0.39019296554471111,{"$f":"F1629*(1-Elteq!$F$6)","v":0.39019296554471111}]
["ANAMET-S",8154320,"M 32","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,0.39948327424815672,{"$f":"F1630*(1-Elteq!$F$6)","v":0.39948327424815672}]
["ANAMET-S",8154400,"M 40","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,0.60387006572395774,{"$f":"F1631*(1-Elteq!$F$6)","v":0.60387006572395774}]
["ANAMET-S",8154500,"M 50","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,0.92903087034455045,{"$f":"F1632*(1-Elteq!$F$6)","v":0.92903087034455045}]
["ANAMET-S",8154630,"M 63","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,1.3470947619995981,{"$f":"F1633*(1-Elteq!$F$6)","v":1.3470947619995981}]
["ANAMET-S",8155070,"PG 7 / - / -","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,0.3344511133240381,{"$f":"F1634*(1-Elteq!$F$6)","v":0.3344511133240381}]
["ANAMET-S",8155090,"PG 9 / M16/ -","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,0.3344511133240381,{"$f":"F1635*(1-Elteq!$F$6)","v":0.3344511133240381}]
["ANAMET-S",8155110,"PG 11 / - / -","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,0.34374142202748365,{"$f":"F1636*(1-Elteq!$F$6)","v":0.34374142202748365}]
["ANAMET-S",8155130,"PG 13,5 / - / -","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,0.36232203943437469,{"$f":"F1637*(1-Elteq!$F$6)","v":0.36232203943437469}]
["ANAMET-S",8155160,"PG 16 / - / 1/2\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,0.37161234813782018,{"$f":"F1638*(1-Elteq!$F$6)","v":0.37161234813782018}]
["ANAMET-S",8155210,"PG 21 /  - / 3/4\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",50,0.39019296554471111,{"$f":"F1639*(1-Elteq!$F$6)","v":0.39019296554471111}]
["ANAMET-S",8155290,"PG 29 / - / 1\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",50,0.39948327424815672,{"$f":"F1640*(1-Elteq!$F$6)","v":0.39948327424815672}]
["ANAMET-S",8155360,"PG 36 / - / 1 1/4\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",50,0.60387006572395774,{"$f":"F1641*(1-Elteq!$F$6)","v":0.60387006572395774}]
["ANAMET-S",8155420,"PG 42 / - / 1 1/2\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",50,0.92903087034455045,{"$f":"F1642*(1-Elteq!$F$6)","v":0.92903087034455045}]
["ANAMET-S",8155480,"PG 48 / - / 2\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",50,1.3470947619995981,{"$f":"F1643*(1-Elteq!$F$6)","v":1.3470947619995981}]
["ANAMET-S",7120149,"M20 x 1,5","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,20.262163282214644,{"$f":"F1644*(1-Elteq!$F$6)","v":20.262163282214644}]
["ANAMET-S",7120159,"M16 x 1,5","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,15.068880716988605,{"$f":"F1645*(1-Elteq!$F$6)","v":15.068880716988605}]
["ANAMET-S",7120169,"M16 x 1,5","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,15.068880716988605,{"$f":"F1646*(1-Elteq!$F$6)","v":15.068880716988605}]
["ANAMET-S",7120179,"M20 x 1,5","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,20.262163282214644,{"$f":"F1647*(1-Elteq!$F$6)","v":20.262163282214644}]
["ANAMET-S",7120209,"M20 x 1,5","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,20.262163282214644,{"$f":"F1648*(1-Elteq!$F$6)","v":20.262163282214644}]
["ANAMET-S",7120259,"M25 x 1,5","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",5,24.117641394144531,{"$f":"F1649*(1-Elteq!$F$6)","v":24.117641394144531}]
["ANAMET-S",7120329,"M32 x 1,5","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",5,30.054148655646209,{"$f":"F1650*(1-Elteq!$F$6)","v":30.054148655646209}]
["ANAMET-S",7120409,"M40 x 1,5","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",2,44.38909498506262,{"$f":"F1651*(1-Elteq!$F$6)","v":44.38909498506262}]
["ANAMET-S",7120509,"M50 x 1,5","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",2,66.490739390559469,{"$f":"F1652*(1-Elteq!$F$6)","v":66.490739390559469}]
["ANAMET-S",7120639,"M63 x 1,5","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",2,94.844761553475152,{"$f":"F1653*(1-Elteq!$F$6)","v":94.844761553475152}]
["ANAMET-S",7129169,"M16 x 1,5","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",10,30.193503286197888,{"$f":"F1654*(1-Elteq!$F$6)","v":30.193503286197888}]
["ANAMET-S",7129179,"M20 x 1,5","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",10,31.122534156542436,{"$f":"F1655*(1-Elteq!$F$6)","v":31.122534156542436}]
["ANAMET-S",7129209,"M20 x 1,5","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",10,34.281239115713909,{"$f":"F1656*(1-Elteq!$F$6)","v":34.281239115713909}]
["ANAMET-S",7129259,"M25 x 1,5","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",5,44.128966341366144,{"$f":"F1657*(1-Elteq!$F$6)","v":44.128966341366144}]
["ANAMET-S",7129329,"M32 x 1,5","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",5,66.239901055566435,{"$f":"F1658*(1-Elteq!$F$6)","v":66.239901055566435}]
["ANAMET-S",7129409,"M40 x 1,5","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",2,85.006324636526372,{"$f":"F1659*(1-Elteq!$F$6)","v":85.006324636526372}]
["ANAMET-S",7129509,"M50 x 1,5","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",2,121.7030440151361,{"$f":"F1660*(1-Elteq!$F$6)","v":121.7030440151361}]
["ANAMET-S",7129639,"M63 x 1,5","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",2,174.65780362477548,{"$f":"F1661*(1-Elteq!$F$6)","v":174.65780362477548}]
["ANAMET-S",7140129,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,15.068880716988605,{"$f":"F1662*(1-Elteq!$F$6)","v":15.068880716988605}]
["ANAMET-S",7140169,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,20.262163282214644,{"$f":"F1663*(1-Elteq!$F$6)","v":20.262163282214644}]
["ANAMET-S",7140209,"NPT 3/4\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",5,24.117641394144531,{"$f":"F1664*(1-Elteq!$F$6)","v":24.117641394144531}]
["ANAMET-S",7140269,"NPT 1\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",5,30.054148655646209,{"$f":"F1665*(1-Elteq!$F$6)","v":30.054148655646209}]
["ANAMET-S",7140359,"NPT 1.1/4\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",2,44.38909498506262,{"$f":"F1666*(1-Elteq!$F$6)","v":44.38909498506262}]
["ANAMET-S",7140409,"NPT 1.1/2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",2,66.490739390559469,{"$f":"F1667*(1-Elteq!$F$6)","v":66.490739390559469}]
["ANAMET-S",7140509,"NPT 2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",2,94.844761553475152,{"$f":"F1668*(1-Elteq!$F$6)","v":94.844761553475152}]
["ANAMET-S",7149129,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",10,30.193503286197888,{"$f":"F1669*(1-Elteq!$F$6)","v":30.193503286197888}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},7149169,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",10,34.281239115713909,{"$f":"F1670*(1-Elteq!$F$6)","v":34.281239115713909}]
["ANAMET-S",7149209,"NPT 3/4\"","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",5,44.128966341366144,{"$f":"F1671*(1-Elteq!$F$6)","v":44.128966341366144}]
["ANAMET-S",7149269,"NPT 1\"","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",5,66.239901055566435,{"$f":"F1672*(1-Elteq!$F$6)","v":66.239901055566435}]
["ANAMET-S",7149359,"NPT 1.1/4\"","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",2,85.006324636526372,{"$f":"F1673*(1-Elteq!$F$6)","v":85.006324636526372}]
["ANAMET-S",7149409,"NPT 1.1/2\"","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",2,121.7030440151361,{"$f":"F1674*(1-Elteq!$F$6)","v":121.7030440151361}]
["ANAMET-S",7149509,"NPT 2\"","Compact fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",2,174.65780362477548,{"$f":"F1675*(1-Elteq!$F$6)","v":174.65780362477548}]
["ANAMET-S","7140129-2","NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,17.660876845249906,{"$f":"F1676*(1-Elteq!$F$6)","v":17.660876845249906}]
["ANAMET-S","7140169-2","NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,22.900610953993166,{"$f":"F1677*(1-Elteq!$F$6)","v":22.900610953993166}]
["ANAMET-S","7140209-2","NPT 3/4\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",5,26.709637522405824,{"$f":"F1678*(1-Elteq!$F$6)","v":26.709637522405824}]
["ANAMET-S","7140269-2","NPT 1\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",5,34.206916646086349,{"$f":"F1679*(1-Elteq!$F$6)","v":34.206916646086349}]
["ANAMET-S","7140359-2","NPT 1.1/4\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",2,49.944699589723022,{"$f":"F1680*(1-Elteq!$F$6)","v":49.944699589723022}]
["ANAMET-S","7140409-2","NPT 1.1/2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",2,74.145953762198573,{"$f":"F1681*(1-Elteq!$F$6)","v":74.145953762198573}]
["ANAMET-S","7140509-2","NPT 2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",2,107.29377521609211,{"$f":"F1682*(1-Elteq!$F$6)","v":107.29377521609211}]
["ANAMET-S","7149129-2","NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,32.785499414459181,{"$f":"F1683*(1-Elteq!$F$6)","v":32.785499414459181}]
["ANAMET-S","7149169-2","NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,36.873235243975202,{"$f":"F1684*(1-Elteq!$F$6)","v":36.873235243975202}]
["ANAMET-S","7149-209-2","NPT 3/4\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",5,46.767414013144666,{"$f":"F1685*(1-Elteq!$F$6)","v":46.767414013144666}]
["ANAMET-S","7149-269-2","NPT 1\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",5,70.392669046006588,{"$f":"F1686*(1-Elteq!$F$6)","v":70.392669046006588}]
["ANAMET-S","7149359-2","NPT 1.1/4\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",2,90.561929241186775,{"$f":"F1687*(1-Elteq!$F$6)","v":90.561929241186775}]
["ANAMET-S","7149409-2","NPT 1.1/2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",2,129.35825838677519,{"$f":"F1688*(1-Elteq!$F$6)","v":129.35825838677519}]
["ANAMET-S","7149509-2","NPT 2\"","Compact fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",2,187.10681728739246,{"$f":"F1689*(1-Elteq!$F$6)","v":187.10681728739246}]
["ANAMET-S",8120149,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,26.170799617605986,{"$f":"F1690*(1-Elteq!$F$6)","v":26.170799617605986}]
["ANAMET-S",8120159,"M16 x 1,5","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,18.915068520215048,{"$f":"F1691*(1-Elteq!$F$6)","v":18.915068520215048}]
["ANAMET-S",8120169,"M16 x 1,5","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,17.725909006174021,{"$f":"F1692*(1-Elteq!$F$6)","v":17.725909006174021}]
["ANAMET-S",8120179,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,24.98164010356496,{"$f":"F1693*(1-Elteq!$F$6)","v":24.98164010356496}]
["ANAMET-S",8120209,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,24.98164010356496,{"$f":"F1694*(1-Elteq!$F$6)","v":24.98164010356496}]
["ANAMET-S",8120259,"M25 x 1,5","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",5,28.725634511053499,{"$f":"F1695*(1-Elteq!$F$6)","v":28.725634511053499}]
["ANAMET-S",8120329,"M 32 x 1,5","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",5,35.433237394941152,{"$f":"F1696*(1-Elteq!$F$6)","v":35.433237394941152}]
["ANAMET-S",8120409,"M40 x 1,5","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",2,73.820792957577979,{"$f":"F1697*(1-Elteq!$F$6)","v":73.820792957577979}]
["ANAMET-S",8124149,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 45° elbow, IP 67",10,44.370514367655723,{"$f":"F1698*(1-Elteq!$F$6)","v":44.370514367655723}]
["ANAMET-S",8124159,"M16 x 1,5","Standard fittings for Sealtite, Stainless steel 304 45° elbow, IP 67",10,31.828597618004292,{"$f":"F1699*(1-Elteq!$F$6)","v":31.828597618004292}]
["ANAMET-S",8124169,"M16 x 1,5","Standard fittings for Sealtite, Stainless steel 304 45° elbow, IP 67",10,30.639438103963268,{"$f":"F1700*(1-Elteq!$F$6)","v":30.639438103963268}]
["ANAMET-S",8124179,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 45° elbow, IP 67",10,43.1813548536147,{"$f":"F1701*(1-Elteq!$F$6)","v":43.1813548536147}]
["ANAMET-S",8124209,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 45° elbow, IP 67",10,43.1813548536147,{"$f":"F1702*(1-Elteq!$F$6)","v":43.1813548536147}]
["ANAMET-S",8124259,"M25 x 1,5","Standard fittings for Sealtite, Stainless steel 304 45° elbow, IP 67",5,49.647409711212774,{"$f":"F1703*(1-Elteq!$F$6)","v":49.647409711212774}]
["ANAMET-S",8127159,"M16 x 1,5","Standard fittings for Sealtite, Stainless steel 304 cablehose, IP 67",10,38.062394758016225,{"$f":"F1704*(1-Elteq!$F$6)","v":38.062394758016225}]
["ANAMET-S",8127169,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 cablehose, IP 67",10,36.873235243975202,{"$f":"F1705*(1-Elteq!$F$6)","v":36.873235243975202}]
["ANAMET-S",8127179,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 cablehose, IP 67",10,39.493102298346834,{"$f":"F1706*(1-Elteq!$F$6)","v":39.493102298346834}]
["ANAMET-S",8127209,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 cablehose, IP 67",10,43.590128436566303,{"$f":"F1707*(1-Elteq!$F$6)","v":43.590128436566303}]
["ANAMET-S",8129149,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",10,44.370514367655723,{"$f":"F1708*(1-Elteq!$F$6)","v":44.370514367655723}]
["ANAMET-S",8129159,"M16 x 1,5","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",10,31.828597618004292,{"$f":"F1709*(1-Elteq!$F$6)","v":31.828597618004292}]
["ANAMET-S",8129169,"M16 x 1,5","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",10,30.639438103963268,{"$f":"F1710*(1-Elteq!$F$6)","v":30.639438103963268}]
["ANAMET-S",8129179,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",10,43.1813548536147,{"$f":"F1711*(1-Elteq!$F$6)","v":43.1813548536147}]
["ANAMET-S",8129209,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",10,43.1813548536147,{"$f":"F1712*(1-Elteq!$F$6)","v":43.1813548536147}]
["ANAMET-S",8129259,"M25 x 1,5","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",5,49.647409711212774,{"$f":"F1713*(1-Elteq!$F$6)","v":49.647409711212774}]
["ANAMET-S",8150115,"3/8\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",50,2.6384476717785232,{"$f":"F1714*(1-Elteq!$F$6)","v":2.6384476717785232}]
["ANAMET-S",8150165,"1/2\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",50,3.1587049591714713,{"$f":"F1715*(1-Elteq!$F$6)","v":3.1587049591714713}]
["ANAMET-S",8150215,"3/4\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",25,3.6975428639713104,{"$f":"F1716*(1-Elteq!$F$6)","v":3.6975428639713104}]
["ANAMET-S",8150295,"1\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",25,4.2178001513642585,{"$f":"F1717*(1-Elteq!$F$6)","v":4.2178001513642585}]
["ANAMET-S",8150365,"1 1/4\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",10,4.5057997211710692,{"$f":"F1718*(1-Elteq!$F$6)","v":4.5057997211710692}]
["ANAMET-S",8150425,"1 1/2\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",10,4.7194768213503169,{"$f":"F1719*(1-Elteq!$F$6)","v":4.7194768213503169}]
["ANAMET-S",8150485,"2\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",10,5.917926644094786,{"$f":"F1720*(1-Elteq!$F$6)","v":5.917926644094786}]
["ANAMET-S",8803169,"NPT 1/2\"","Compact fittings for Sealtite, Locknut, stainless steel 304",100,1.6536749492132996,{"$f":"F1721*(1-Elteq!$F$6)","v":1.6536749492132996}]
["ANAMET-S",8803209,"NPT 3/4\"","Compact fittings for Sealtite, Locknut, stainless steel 304",50,2.4061899541923855,{"$f":"F1722*(1-Elteq!$F$6)","v":2.4061899541923855}]
["ANAMET-S",8803269,"NPT 1 \"","Compact fittings for Sealtite, Locknut, stainless steel 304",50,4.2828323122883774,{"$f":"F1723*(1-Elteq!$F$6)","v":4.2828323122883774}]
["ANAMET-S",8803359,"NPT 1 1/4\"","Compact fittings for Sealtite, Locknut, stainless steel 304",20,4.765928364867543,{"$f":"F1724*(1-Elteq!$F$6)","v":4.765928364867543}]
["ANAMET-S",8803409,"NPT 1 1/2\"","Compact fittings for Sealtite, Locknut, stainless steel 304",20,6.2245068313084877,{"$f":"F1725*(1-Elteq!$F$6)","v":6.2245068313084877}]
["ANAMET-S",8803509,"NPT 2\"","Compact fittings for Sealtite, Locknut, stainless steel 304",20,9.6990822863971058,{"$f":"F1726*(1-Elteq!$F$6)","v":9.6990822863971058}]
["ANAMET-S",8100119,"PG 11","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,17.725909006174021,{"$f":"F1727*(1-Elteq!$F$6)","v":17.725909006174021}]
["ANAMET-S",8100129,"PG 11","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,18.915068520215048,{"$f":"F1728*(1-Elteq!$F$6)","v":18.915068520215048}]
["ANAMET-S",8100139,"PG 13,5","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,17.725909006174021,{"$f":"F1729*(1-Elteq!$F$6)","v":17.725909006174021}]
["ANAMET-S",8100149,"PG 13,5","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,18.915068520215048,{"$f":"F1730*(1-Elteq!$F$6)","v":18.915068520215048}]
["ANAMET-S",8100169,"PG 16","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,24.98164010356496,{"$f":"F1731*(1-Elteq!$F$6)","v":24.98164010356496}]
["ANAMET-S",8100219,"PG 21","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",5,28.725634511053499,{"$f":"F1732*(1-Elteq!$F$6)","v":28.725634511053499}]
["ANAMET-S",8100299,"PG 29","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",5,35.433237394941152,{"$f":"F1733*(1-Elteq!$F$6)","v":35.433237394941152}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8100369,"PG 36","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",2,73.820792957577979,{"$f":"F1734*(1-Elteq!$F$6)","v":73.820792957577979}]
["ANAMET-S",8100429,"PG 42","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",2,118.30279102967505,{"$f":"F1735*(1-Elteq!$F$6)","v":118.30279102967505}]
["ANAMET-S",8100489,"PG 48","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",2,180.28773069906345,{"$f":"F1736*(1-Elteq!$F$6)","v":180.28773069906345}]
["ANAMET-S",8109119,"PG 11","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",10,30.639438103963268,{"$f":"F1737*(1-Elteq!$F$6)","v":30.639438103963268}]
["ANAMET-S",8109129,"PG 11","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",10,31.828597618004292,{"$f":"F1738*(1-Elteq!$F$6)","v":31.828597618004292}]
["ANAMET-S",8109169,"PG 16","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",10,43.1813548536147,{"$f":"F1739*(1-Elteq!$F$6)","v":43.1813548536147}]
["ANAMET-S",8109219,"PG 21","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",5,49.647409711212774,{"$f":"F1740*(1-Elteq!$F$6)","v":49.647409711212774}]
["ANAMET-S",8109299,"PG 29","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",5,55.667529751045464,{"$f":"F1741*(1-Elteq!$F$6)","v":55.667529751045464}]
["ANAMET-S",8140119,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,19.751196303525145,{"$f":"F1742*(1-Elteq!$F$6)","v":19.751196303525145}]
["ANAMET-S",8140129,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,18.562036789484118,{"$f":"F1743*(1-Elteq!$F$6)","v":18.562036789484118}]
["ANAMET-S",8140169,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,26.170799617605986,{"$f":"F1744*(1-Elteq!$F$6)","v":26.170799617605986}]
["ANAMET-S",8140209,"NPT 3/4\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",5,30.091309890459989,{"$f":"F1745*(1-Elteq!$F$6)","v":30.091309890459989}]
["ANAMET-S",8140269,"NPT 1 \"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",5,33.742401210914068,{"$f":"F1746*(1-Elteq!$F$6)","v":33.742401210914068}]
["ANAMET-S",8144119,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 45° elbow, IP 67",10,33.222143923521124,{"$f":"F1747*(1-Elteq!$F$6)","v":33.222143923521124}]
["ANAMET-S",8144129,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 45° elbow, IP 67",10,32.032984409480093,{"$f":"F1748*(1-Elteq!$F$6)","v":32.032984409480093}]
["ANAMET-S",8144169,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 45° elbow, IP 67",10,45.160190607448598,{"$f":"F1749*(1-Elteq!$F$6)","v":45.160190607448598}]
["ANAMET-S",8144209,"NPT 3/4\"","Standard fittings for Sealtite, Stainless steel 304 45° elbow, IP 67",5,51.904954726150031,{"$f":"F1750*(1-Elteq!$F$6)","v":51.904954726150031}]
["ANAMET-S",8149119,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",10,33.222143923521124,{"$f":"F1751*(1-Elteq!$F$6)","v":33.222143923521124}]
["ANAMET-S",8149129,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",10,32.032984409480093,{"$f":"F1752*(1-Elteq!$F$6)","v":32.032984409480093}]
["ANAMET-S",8149169,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",10,45.160190607448598,{"$f":"F1753*(1-Elteq!$F$6)","v":45.160190607448598}]
["ANAMET-S",8149209,"NPT 3/4\"","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",5,51.904954726150031,{"$f":"F1754*(1-Elteq!$F$6)","v":51.904954726150031}]
["ANAMET-S",8149269,"NPT 1 \"","Standard fittings for Sealtite, Stainless steel 304 90° elbow, IP 67",5,58.203784027086087,{"$f":"F1755*(1-Elteq!$F$6)","v":58.203784027086087}]
["ANAMET-S",8150119,"3/8\"","Compact fittings for Sealtite, Ferrule, stainless steel 316",10,10.971854578769141,{"$f":"F1756*(1-Elteq!$F$6)","v":10.971854578769141}]
["ANAMET-S",8150169,"1/2\"","Compact fittings for Sealtite, Ferrule, stainless steel 316",10,14.994558247361045,{"$f":"F1757*(1-Elteq!$F$6)","v":14.994558247361045}]
["ANAMET-S",8150219,"3/4\"","Compact fittings for Sealtite, Ferrule, stainless steel 316",5,19.351713029276983,{"$f":"F1758*(1-Elteq!$F$6)","v":19.351713029276983}]
["ANAMET-S",8150299,"1\"","Compact fittings for Sealtite, Ferrule, stainless steel 316",5,24.888737016530506,{"$f":"F1759*(1-Elteq!$F$6)","v":24.888737016530506}]
["ANAMET-S",7121149,"M20 x 1,5","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",10,26.338025174268004,{"$f":"F1760*(1-Elteq!$F$6)","v":26.338025174268004}]
["ANAMET-S",7121159,"M16 x 1,5","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",10,19.593261055566568,{"$f":"F1761*(1-Elteq!$F$6)","v":19.593261055566568}]
["ANAMET-S",7121169,"M16 x 1,5","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",10,19.593261055566568,{"$f":"F1762*(1-Elteq!$F$6)","v":19.593261055566568}]
["ANAMET-S",7121179,"M20 x 1,5","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",10,26.338025174268004,{"$f":"F1763*(1-Elteq!$F$6)","v":26.338025174268004}]
["ANAMET-S",7121209,"M20 x 1,5","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",10,26.338025174268004,{"$f":"F1764*(1-Elteq!$F$6)","v":26.338025174268004}]
["ANAMET-S",7121259,"M25 x 1,5","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",5,31.354791874128576,{"$f":"F1765*(1-Elteq!$F$6)","v":31.354791874128576}]
["ANAMET-S",7121329,"M32 x 1,5","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",5,39.075038406691796,{"$f":"F1766*(1-Elteq!$F$6)","v":39.075038406691796}]
["ANAMET-S",7121409,"M40 x 1,5","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",2,57.702107357100026,{"$f":"F1767*(1-Elteq!$F$6)","v":57.702107357100026}]
["ANAMET-S",7121509,"M50 x 1,5","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",2,86.437032176856974,{"$f":"F1768*(1-Elteq!$F$6)","v":86.437032176856974}]
["ANAMET-S",7121639,"M63 x 1,5","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",2,123.30097711212873,{"$f":"F1769*(1-Elteq!$F$6)","v":123.30097711212873}]
["ANAMET-S",7125169,"M16 x 1,5","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",10,40.765874590718873,{"$f":"F1770*(1-Elteq!$F$6)","v":40.765874590718873}]
["ANAMET-S",7125179,"M20 x 1,5","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",10,42.020066265684008,{"$f":"F1771*(1-Elteq!$F$6)","v":42.020066265684008}]
["ANAMET-S",7125209,"M20 x 1,5","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",10,46.284317960565502,{"$f":"F1772*(1-Elteq!$F$6)","v":46.284317960565502}]
["ANAMET-S",7125259,"M25 x 1,5","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",5,59.578749715196011,{"$f":"F1773*(1-Elteq!$F$6)","v":59.578749715196011}]
["ANAMET-S",7125329,"M32 x 1,5","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",5,89.428511579366429,{"$f":"F1774*(1-Elteq!$F$6)","v":89.428511579366429}]
["ANAMET-S",7125409,"M40 x 1,5","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",2,114.7631834136623,{"$f":"F1775*(1-Elteq!$F$6)","v":114.7631834136623}]
["ANAMET-S",7125509,"M50 x 1,5","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",2,164.29910942043372,{"$f":"F1776*(1-Elteq!$F$6)","v":164.29910942043372}]
["ANAMET-S",7125639,"M63 x 1,5","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",2,235.78803489344691,{"$f":"F1777*(1-Elteq!$F$6)","v":235.78803489344691}]
["ANAMET-S",7141129,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",10,19.593261055566568,{"$f":"F1778*(1-Elteq!$F$6)","v":19.593261055566568}]
["ANAMET-S",7141169,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",10,26.338025174268004,{"$f":"F1779*(1-Elteq!$F$6)","v":26.338025174268004}]
["ANAMET-S",7141209,"NPT 3/4\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",5,31.354791874128576,{"$f":"F1780*(1-Elteq!$F$6)","v":31.354791874128576}]
["ANAMET-S",7141269,"NPT 1\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",5,39.075038406691796,{"$f":"F1781*(1-Elteq!$F$6)","v":39.075038406691796}]
["ANAMET-S",7141359,"NPT 1.1/4\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",2,57.702107357100026,{"$f":"F1782*(1-Elteq!$F$6)","v":57.702107357100026}]
["ANAMET-S",7141409,"NPT 1.1/2\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",2,86.437032176856974,{"$f":"F1783*(1-Elteq!$F$6)","v":86.437032176856974}]
["ANAMET-S",7141509,"NPT 2\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",2,123.30097711212873,{"$f":"F1784*(1-Elteq!$F$6)","v":123.30097711212873}]
["ANAMET-S",7145129,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",10,40.765874590718873,{"$f":"F1785*(1-Elteq!$F$6)","v":40.765874590718873}]
["ANAMET-S",7145169,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",10,46.284317960565502,{"$f":"F1786*(1-Elteq!$F$6)","v":46.284317960565502}]
["ANAMET-S",7145209,"NPT 3/4\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",5,59.578749715196011,{"$f":"F1787*(1-Elteq!$F$6)","v":59.578749715196011}]
["ANAMET-S",7145269,"NPT 1\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",5,89.428511579366429,{"$f":"F1788*(1-Elteq!$F$6)","v":89.428511579366429}]
["ANAMET-S",7145359,"NPT 1.1/4\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",2,114.7631834136623,{"$f":"F1789*(1-Elteq!$F$6)","v":114.7631834136623}]
["ANAMET-S",7145409,"NPT 1.1/2\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",2,164.29910942043372,{"$f":"F1790*(1-Elteq!$F$6)","v":164.29910942043372}]
["ANAMET-S",7145509,"NPT 2\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",2,235.78803489344691,{"$f":"F1791*(1-Elteq!$F$6)","v":235.78803489344691}]
["ANAMET-S",71411292,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",10,22.185257183827861,{"$f":"F1792*(1-Elteq!$F$6)","v":22.185257183827861}]
["ANAMET-S",71411692,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",10,28.930021302529301,{"$f":"F1793*(1-Elteq!$F$6)","v":28.930021302529301}]
["ANAMET-S",71412092,"NPT 3/4\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",5,33.993239545907102,{"$f":"F1794*(1-Elteq!$F$6)","v":33.993239545907102}]
["ANAMET-S",71412692,"NPT 1\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",5,43.227806397131928,{"$f":"F1795*(1-Elteq!$F$6)","v":43.227806397131928}]
["ANAMET-S",71413592,"NPT 1.1/4\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",2,63.257711961760435,{"$f":"F1796*(1-Elteq!$F$6)","v":63.257711961760435}]
["ANAMET-S",71414092,"NPT 1.1/2\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",2,94.092246548496064,{"$f":"F1797*(1-Elteq!$F$6)","v":94.092246548496064}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},71415092,"NPT 2\"","Compact fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",2,135.74999077474573,{"$f":"F1798*(1-Elteq!$F$6)","v":135.74999077474573}]
["ANAMET-S",71451292,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",10,43.357870718980166,{"$f":"F1799*(1-Elteq!$F$6)","v":43.357870718980166}]
["ANAMET-S",71451692,"NPT 1/2\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",10,48.876314088826796,{"$f":"F1800*(1-Elteq!$F$6)","v":48.876314088826796}]
["ANAMET-S",71452092,"NPT 3/4\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",5,62.217197386974547,{"$f":"F1801*(1-Elteq!$F$6)","v":62.217197386974547}]
["ANAMET-S",71452692,"NPT 1\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",5,93.581279569806568,{"$f":"F1802*(1-Elteq!$F$6)","v":93.581279569806568}]
["ANAMET-S",71453592,"NPT 1.1/4\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",2,120.31878801832271,{"$f":"F1803*(1-Elteq!$F$6)","v":120.31878801832271}]
["ANAMET-S",71454092,"NPT 1.1/2\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",2,171.95432379207284,{"$f":"F1804*(1-Elteq!$F$6)","v":171.95432379207284}]
["ANAMET-S",71455092,"NPT 2\"","Compact fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",2,248.23704855606388,{"$f":"F1805*(1-Elteq!$F$6)","v":248.23704855606388}]
["ANAMET-S",8101169,"PG 16","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",10,28.892860067715521,{"$f":"F1806*(1-Elteq!$F$6)","v":28.892860067715521}]
["ANAMET-S",8101219,"PG 21","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",5,43.02341960565613,{"$f":"F1807*(1-Elteq!$F$6)","v":43.02341960565613}]
["ANAMET-S",8101299,"PG 29","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",5,57.469849639513889,{"$f":"F1808*(1-Elteq!$F$6)","v":57.469849639513889}]
["ANAMET-S",8121169,"M16 x 1,5","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",10,25.343962142999338,{"$f":"F1809*(1-Elteq!$F$6)","v":25.343962142999338}]
["ANAMET-S",8121209,"M20 x 1,5","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",10,28.892860067715521,{"$f":"F1810*(1-Elteq!$F$6)","v":28.892860067715521}]
["ANAMET-S",8121259,"M25 x 1,5","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",5,43.02341960565613,{"$f":"F1811*(1-Elteq!$F$6)","v":43.02341960565613}]
["ANAMET-S",8121329,"M32 x 1,5","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",5,57.469849639513889,{"$f":"F1812*(1-Elteq!$F$6)","v":57.469849639513889}]
["ANAMET-S",8141129,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",10,25.343962142999338,{"$f":"F1813*(1-Elteq!$F$6)","v":25.343962142999338}]
["ANAMET-S",8141169,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",10,28.892860067715521,{"$f":"F1814*(1-Elteq!$F$6)","v":28.892860067715521}]
["ANAMET-S",8141209,"NPT 3/4\"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",5,43.02341960565613,{"$f":"F1815*(1-Elteq!$F$6)","v":43.02341960565613}]
["ANAMET-S",8141269,"NPT 1 \"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",5,57.469849639513889,{"$f":"F1816*(1-Elteq!$F$6)","v":57.469849639513889}]
["ANAMET-S",8145129,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",10,57.284043465444974,{"$f":"F1817*(1-Elteq!$F$6)","v":57.284043465444974}]
["ANAMET-S",8145169,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",10,66.35138476000779,{"$f":"F1818*(1-Elteq!$F$6)","v":66.35138476000779}]
["ANAMET-S",8145209,"NPT 3/4\"","Standard fittings for Sealtite, Stainless steel 316 90° elbow, IP 67",5,79.348526636128057,{"$f":"F1819*(1-Elteq!$F$6)","v":79.348526636128057}]
["ANAMET-S",8150115,"3/8\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",50,2.6384476717785232,{"$f":"F1820*(1-Elteq!$F$6)","v":2.6384476717785232}]
["ANAMET-S",8150119,"3/8\"","Compact fittings for Sealtite, Ferrule, stainless steel 316",10,10.971854578769141,{"$f":"F1821*(1-Elteq!$F$6)","v":10.971854578769141}]
["ANAMET-S",8150165,"1/2\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",50,3.1587049591714713,{"$f":"F1822*(1-Elteq!$F$6)","v":3.1587049591714713}]
["ANAMET-S",8150169,"1/2\"","Compact fittings for Sealtite, Ferrule, stainless steel 316",10,14.994558247361045,{"$f":"F1823*(1-Elteq!$F$6)","v":14.994558247361045}]
["ANAMET-S",8150215,"3/4\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",25,3.6975428639713104,{"$f":"F1824*(1-Elteq!$F$6)","v":3.6975428639713104}]
["ANAMET-S",8150219,"3/4\"","Compact fittings for Sealtite, Ferrule, stainless steel 316",5,19.351713029276983,{"$f":"F1825*(1-Elteq!$F$6)","v":19.351713029276983}]
["ANAMET-S",8150295,"1\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",25,4.2178001513642585,{"$f":"F1826*(1-Elteq!$F$6)","v":4.2178001513642585}]
["ANAMET-S",8150299,"1\"","Compact fittings for Sealtite, Ferrule, stainless steel 316",5,24.888737016530506,{"$f":"F1827*(1-Elteq!$F$6)","v":24.888737016530506}]
["ANAMET-S",8150365,"1 1/4\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",10,4.5057997211710692,{"$f":"F1828*(1-Elteq!$F$6)","v":4.5057997211710692}]
["ANAMET-S",8150425,"1 1/2\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",10,4.7194768213503169,{"$f":"F1829*(1-Elteq!$F$6)","v":4.7194768213503169}]
["ANAMET-S",8150485,"2\"","Compact fittings for Sealtite, Ferrule, stainless steel 304",10,5.917926644094786,{"$f":"F1830*(1-Elteq!$F$6)","v":5.917926644094786}]
["ANAMET-S",8803169,"NPT 1/2\"","Compact fittings for Sealtite, Locknut, stainless steel 304",100,1.6536749492132996,{"$f":"F1831*(1-Elteq!$F$6)","v":1.6536749492132996}]
["ANAMET-S",8803209,"NPT 3/4\"","Compact fittings for Sealtite, Locknut, stainless steel 304",50,2.4061899541923855,{"$f":"F1832*(1-Elteq!$F$6)","v":2.4061899541923855}]
["ANAMET-S",8803269,"NPT 1 \"","Compact fittings for Sealtite, Locknut, stainless steel 304",50,4.2828323122883774,{"$f":"F1833*(1-Elteq!$F$6)","v":4.2828323122883774}]
["ANAMET-S",8803359,"NPT 1 1/4\"","Compact fittings for Sealtite, Locknut, stainless steel 304",20,4.765928364867543,{"$f":"F1834*(1-Elteq!$F$6)","v":4.765928364867543}]
["ANAMET-S",8803409,"NPT 1 1/2\"","Compact fittings for Sealtite, Locknut, stainless steel 304",20,6.2245068313084877,{"$f":"F1835*(1-Elteq!$F$6)","v":6.2245068313084877}]
["ANAMET-S",8803509,"NPT 2\"","Compact fittings for Sealtite, Locknut, stainless steel 304",20,9.6990822863971058,{"$f":"F1836*(1-Elteq!$F$6)","v":9.6990822863971058}]
["ANAMET-S",7189400,"M40 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",2,37.374911913961263,{"$f":"F1837*(1-Elteq!$F$6)","v":37.374911913961263}]
["ANAMET-S",7189500,"M50 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",2,50.372053790081523,{"$f":"F1838*(1-Elteq!$F$6)","v":50.372053790081523}]
["ANAMET-S",7189630,"M63 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",2,75.613822537342955,{"$f":"F1839*(1-Elteq!$F$6)","v":75.613822537342955}]
["ANAMET-S",8189161,"M16 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",10,13.470947619995981,{"$f":"F1840*(1-Elteq!$F$6)","v":13.470947619995981}]
["ANAMET-S",8189201,"M20 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",10,17.18707110137418,{"$f":"F1841*(1-Elteq!$F$6)","v":17.18707110137418}]
["ANAMET-S",8189251,"M25 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",5,21.739322366062478,{"$f":"F1842*(1-Elteq!$F$6)","v":21.739322366062478}]
["ANAMET-S",8189321,"M32 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",5,37.904459510057656,{"$f":"F1843*(1-Elteq!$F$6)","v":37.904459510057656}]
["ANAMET-S",8189401,"M40 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",2,62.709583748257153,{"$f":"F1844*(1-Elteq!$F$6)","v":62.709583748257153}]
["ANAMET-S",8189501,"M50 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",2,81.290201155148168,{"$f":"F1845*(1-Elteq!$F$6)","v":81.290201155148168}]
["ANAMET-S",8189631,"M63 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",2,127.2772292372034,{"$f":"F1846*(1-Elteq!$F$6)","v":127.2772292372034}]
["ANAMET-S",8192129,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67",10,48.913475323640576,{"$f":"F1847*(1-Elteq!$F$6)","v":48.913475323640576}]
["ANAMET-S",8192169,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67",10,64.196033140808439,{"$f":"F1848*(1-Elteq!$F$6)","v":64.196033140808439}]
["ANAMET-S",8195129,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67",10,48.913475323640576,{"$f":"F1849*(1-Elteq!$F$6)","v":48.913475323640576}]
["ANAMET-S",8195169,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67",10,64.196033140808439,{"$f":"F1850*(1-Elteq!$F$6)","v":64.196033140808439}]
["ANAMET-S",8320169,"M 16 x 1,5","Food grade fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",10,40.951680764787774,{"$f":"F1851*(1-Elteq!$F$6)","v":40.951680764787774}]
["ANAMET-S",8320209,"M 20 x 1,5","Food grade fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",10,40.951680764787774,{"$f":"F1852*(1-Elteq!$F$6)","v":40.951680764787774}]
["ANAMET-S",8320259,"M 25 x 1,5","Food grade fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",5,55.39811079864554,{"$f":"F1853*(1-Elteq!$F$6)","v":55.39811079864554}]
["ANAMET-S",8320329,"M 32 x 1,5","Food grade fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",5,81.949813073092784,{"$f":"F1854*(1-Elteq!$F$6)","v":81.949813073092784}]
["ANAMET-S",8320409,"M 40 x 1,5","Food grade fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",2,118.57220998207495,{"$f":"F1855*(1-Elteq!$F$6)","v":118.57220998207495}]
["ANAMET-S",8320509,"M 50 x 1,5","Food grade fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",2,186.07559302131,{"$f":"F1856*(1-Elteq!$F$6)","v":186.07559302131}]
["ANAMET-S",8320639,"M 63 x 1,5","Food grade fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,415.55550830511743,{"$f":"F1857*(1-Elteq!$F$6)","v":415.55550830511743}]
["ANAMET-S",8382209,"NPT 3/4\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67",5,99.034690778729058,{"$f":"F1858*(1-Elteq!$F$6)","v":99.034690778729058}]
["ANAMET-S",8382269,"NPT 1\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67",5,152.10093409280981,{"$f":"F1859*(1-Elteq!$F$6)","v":152.10093409280981}]
["ANAMET-S",8385209,"NPT 3/4\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67",5,99.034690778729058,{"$f":"F1860*(1-Elteq!$F$6)","v":99.034690778729058}]
["ANAMET-S",8385269,"NPT 1\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67",5,152.10093409280981,{"$f":"F1861*(1-Elteq!$F$6)","v":152.10093409280981}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},2930400,"M 50 x 1,5","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,12.43972335391353,{"$f":"F1862*(1-Elteq!$F$6)","v":12.43972335391353}]
["ANAMET-S",2930500,"M 63 x 1,5","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,17.38216758414654,{"$f":"F1863*(1-Elteq!$F$6)","v":17.38216758414654}]
["ANAMET-S",2940630,"NPT 2 1/2\"","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,32.701886636128179,{"$f":"F1864*(1-Elteq!$F$6)","v":32.701886636128179}]
["ANAMET-S",2940750,"NPT 3\"","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,44.38909498506262,{"$f":"F1865*(1-Elteq!$F$6)","v":44.38909498506262}]
["ANAMET-S",2940990,"NPT 4\"","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,67.717060139414286,{"$f":"F1866*(1-Elteq!$F$6)","v":67.717060139414286}]
["ANAMET-S",2949630,"NPT 2 1/2\"","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,70.736410468034066,{"$f":"F1867*(1-Elteq!$F$6)","v":70.736410468034066}]
["ANAMET-S",2949750,"NPT 3\"","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,97.288112742481317,{"$f":"F1868*(1-Elteq!$F$6)","v":97.288112742481317}]
["ANAMET-S",2949990,"NPT 4\"","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,113.60189482573163,{"$f":"F1869*(1-Elteq!$F$6)","v":113.60189482573163}]
["ANAMET-S",2950120,"M 16 x 1,5","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",25,6.1037328181636967,{"$f":"F1870*(1-Elteq!$F$6)","v":6.1037328181636967}]
["ANAMET-S",2950160,"M 20 x 1,5","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",25,6.5496676359290804,{"$f":"F1871*(1-Elteq!$F$6)","v":6.5496676359290804}]
["ANAMET-S",2950200,"M 25 x 1,5","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",25,9.689791977693659,{"$f":"F1872*(1-Elteq!$F$6)","v":9.689791977693659}]
["ANAMET-S",2950260,"M 32 x 1,5","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",10,13.861140585540692,{"$f":"F1873*(1-Elteq!$F$6)","v":13.861140585540692}]
["ANAMET-S",2954120,"M16 x 1,5","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",25,10.637403465445102,{"$f":"F1874*(1-Elteq!$F$6)","v":10.637403465445102}]
["ANAMET-S",2954160,"M20 x 1,5","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",25,12.58836829316866,{"$f":"F1875*(1-Elteq!$F$6)","v":12.58836829316866}]
["ANAMET-S",2954200,"M25 x 1,5","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,18.942939446325383,{"$f":"F1876*(1-Elteq!$F$6)","v":18.942939446325383}]
["ANAMET-S",2954260,"M32 x 1,5","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",5,34.83865763792064,{"$f":"F1877*(1-Elteq!$F$6)","v":34.83865763792064}]
["ANAMET-S",2959120,"M16 x 1,5","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",25,10.637403465445102,{"$f":"F1878*(1-Elteq!$F$6)","v":10.637403465445102}]
["ANAMET-S",2959160,"M20 x 1,5","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",25,12.58836829316866,{"$f":"F1879*(1-Elteq!$F$6)","v":12.58836829316866}]
["ANAMET-S",2959200,"M25 x 1,5","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,18.942939446325383,{"$f":"F1880*(1-Elteq!$F$6)","v":18.942939446325383}]
["ANAMET-S",2959260,"M32 x 1,5","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",5,34.83865763792064,{"$f":"F1881*(1-Elteq!$F$6)","v":34.83865763792064}]
["ANAMET-S",2980120,"NPT 1/2\"","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",25,6.5496676359290804,{"$f":"F1882*(1-Elteq!$F$6)","v":6.5496676359290804}]
["ANAMET-S",2980160,"NPT 1/2\"","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",25,6.5496676359290804,{"$f":"F1883*(1-Elteq!$F$6)","v":6.5496676359290804}]
["ANAMET-S",2980200,"NPT 3/4\"","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",25,9.5783082732523148,{"$f":"F1884*(1-Elteq!$F$6)","v":9.5783082732523148}]
["ANAMET-S",2980260,"NPT 1\"","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",5,14.836622999402472,{"$f":"F1885*(1-Elteq!$F$6)","v":14.836622999402472}]
["ANAMET-S",2980350,"NPT 1 1/4\"","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",5,24.387060346544448,{"$f":"F1886*(1-Elteq!$F$6)","v":24.387060346544448}]
["ANAMET-S",2980400,"NPT 1 1/2\"","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",2,37.031170491933779,{"$f":"F1887*(1-Elteq!$F$6)","v":37.031170491933779}]
["ANAMET-S",2980500,"NPT 2\"","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,59.123524588727193,{"$f":"F1888*(1-Elteq!$F$6)","v":59.123524588727193}]
["ANAMET-S",2980630,"NPT 2 1/2\"","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,301.96290378808919,{"$f":"F1889*(1-Elteq!$F$6)","v":301.96290378808919}]
["ANAMET-S",2980750,"NPT 3\"","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,334.57188733718289,{"$f":"F1890*(1-Elteq!$F$6)","v":334.57188733718289}]
["ANAMET-S",2980990,"NPT 4\"","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,389.79348227046302,{"$f":"F1891*(1-Elteq!$F$6)","v":389.79348227046302}]
["ANAMET-S",2984120,"NPT 1/2\"","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",25,10.823209639514012,{"$f":"F1892*(1-Elteq!$F$6)","v":10.823209639514012}]
["ANAMET-S",2984160,"NPT 1/2\"","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",25,10.823209639514012,{"$f":"F1893*(1-Elteq!$F$6)","v":10.823209639514012}]
["ANAMET-S",2984200,"NPT 3/4\"","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",25,16.369523935470976,{"$f":"F1894*(1-Elteq!$F$6)","v":16.369523935470976}]
["ANAMET-S",2984260,"NPT 1\"","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",5,31.011050452101095,{"$f":"F1895*(1-Elteq!$F$6)","v":31.011050452101095}]
["ANAMET-S",2984350,"NPT 1 1/4\"","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",5,50.232699159529837,{"$f":"F1896*(1-Elteq!$F$6)","v":50.232699159529837}]
["ANAMET-S",2984400,"NPT 1 1/2\"","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",2,73.244793817964364,{"$f":"F1897*(1-Elteq!$F$6)","v":73.244793817964364}]
["ANAMET-S",2984500,"NPT 2\"","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,95.262825445130204,{"$f":"F1898*(1-Elteq!$F$6)","v":95.262825445130204}]
["ANAMET-S",2984630,"NPT 2 1/2\"","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,451.99209904003067,{"$f":"F1899*(1-Elteq!$F$6)","v":451.99209904003067}]
["ANAMET-S",2984750,"NPT 3\"","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,545.17389533558912,{"$f":"F1900*(1-Elteq!$F$6)","v":545.17389533558912}]
["ANAMET-S",2984990,"NPT 4\"","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,630.10589750248789,{"$f":"F1901*(1-Elteq!$F$6)","v":630.10589750248789}]
["ANAMET-S",2986120,"NPT 1/2\"","Steel fittings for Sealtite, Straight fixed with female thread, IP 67",25,7.8967623979286792,{"$f":"F1902*(1-Elteq!$F$6)","v":7.8967623979286792}]
["ANAMET-S",2986160,"NPT 1/2\"","Steel fittings for Sealtite, Straight fixed with female thread, IP 67",25,8.2126328938458251,{"$f":"F1903*(1-Elteq!$F$6)","v":8.2126328938458251}]
["ANAMET-S",2986200,"NPT 3/4\"","Steel fittings for Sealtite, Straight fixed with female thread, IP 67",25,11.25985414857595,{"$f":"F1904*(1-Elteq!$F$6)","v":11.25985414857595}]
["ANAMET-S",2986260,"NPT 1\"","Steel fittings for Sealtite, Straight fixed with female thread, IP 67",5,15.524105843457438,{"$f":"F1905*(1-Elteq!$F$6)","v":15.524105843457438}]
["ANAMET-S",2990110,"PG 11","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",25,6.1037328181636967,{"$f":"F1906*(1-Elteq!$F$6)","v":6.1037328181636967}]
["ANAMET-S",2990130,"PG 13,5","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",25,6.1037328181636967,{"$f":"F1907*(1-Elteq!$F$6)","v":6.1037328181636967}]
["ANAMET-S",2990160,"PG 16","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",25,6.5496676359290804,{"$f":"F1908*(1-Elteq!$F$6)","v":6.5496676359290804}]
["ANAMET-S",2990200,"PG 21","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",25,9.689791977693659,{"$f":"F1909*(1-Elteq!$F$6)","v":9.689791977693659}]
["ANAMET-S",2990260,"PG 29","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",5,14.530042812188769,{"$f":"F1910*(1-Elteq!$F$6)","v":14.530042812188769}]
["ANAMET-S",2990350,"PG 36","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",5,26.412347643895568,{"$f":"F1911*(1-Elteq!$F$6)","v":26.412347643895568}]
["ANAMET-S",2990400,"PG 42","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",2,35.40536646883082,{"$f":"F1912*(1-Elteq!$F$6)","v":35.40536646883082}]
["ANAMET-S",2990500,"PG 48","Steel fittings for Sealtite, Straight fixed with male thread, IP 67",1,58.742621931885921,{"$f":"F1913*(1-Elteq!$F$6)","v":58.742621931885921}]
["ANAMET-S",2994110,"PG 11","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",25,11.15766075283805,{"$f":"F1914*(1-Elteq!$F$6)","v":11.15766075283805}]
["ANAMET-S",2994130,"PG 13,5","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",25,11.15766075283805,{"$f":"F1915*(1-Elteq!$F$6)","v":11.15766075283805}]
["ANAMET-S",2994160,"PG 16","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",25,12.932109715196141,{"$f":"F1916*(1-Elteq!$F$6)","v":12.932109715196141}]
["ANAMET-S",2994200,"PG 21","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,16.954813383788046,{"$f":"F1917*(1-Elteq!$F$6)","v":16.954813383788046}]
["ANAMET-S",2994260,"PG 29","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",5,30.156342051384108,{"$f":"F1918*(1-Elteq!$F$6)","v":30.156342051384108}]
["ANAMET-S",2994350,"PG 36","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",5,44.231159737104043,{"$f":"F1919*(1-Elteq!$F$6)","v":44.231159737104043}]
["ANAMET-S",2994400,"PG 42","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",2,63.991646349332626,{"$f":"F1920*(1-Elteq!$F$6)","v":63.991646349332626}]
["ANAMET-S",2994500,"PG 48","Steel fittings for Sealtite, 45° elbow fixed with male thread, IP 67",1,92.670829316868904,{"$f":"F1921*(1-Elteq!$F$6)","v":92.670829316868904}]
["ANAMET-S",2999110,"PG 11","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",25,11.15766075283805,{"$f":"F1922*(1-Elteq!$F$6)","v":11.15766075283805}]
["ANAMET-S",2999130,"PG 13,5","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",25,11.15766075283805,{"$f":"F1923*(1-Elteq!$F$6)","v":11.15766075283805}]
["ANAMET-S",2999160,"PG 16","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",25,12.932109715196141,{"$f":"F1924*(1-Elteq!$F$6)","v":12.932109715196141}]
["ANAMET-S",2999200,"PG 21","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",10,16.954813383788046,{"$f":"F1925*(1-Elteq!$F$6)","v":16.954813383788046}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},2999260,"PG 29","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",5,30.156342051384108,{"$f":"F1926*(1-Elteq!$F$6)","v":30.156342051384108}]
["ANAMET-S",2999400,"PG 42","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,63.991646349332626,{"$f":"F1927*(1-Elteq!$F$6)","v":63.991646349332626}]
["ANAMET-S",2999500,"PG 48","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,92.670829316868904,{"$f":"F1928*(1-Elteq!$F$6)","v":92.670829316868904}]
["ANAMET-S",2972120,"-","Steel fittings for Sealtite, Ferrule, galvanised steel",50,1.8394811232822097,{"$f":"F1929*(1-Elteq!$F$6)","v":1.8394811232822097}]
["ANAMET-S",2972160,"-","Steel fittings for Sealtite, Ferrule, galvanised steel",25,1.8394811232822097,{"$f":"F1930*(1-Elteq!$F$6)","v":1.8394811232822097}]
["ANAMET-S",2972200,"-","Steel fittings for Sealtite, Ferrule, galvanised steel",25,2.0624485321649022,{"$f":"F1931*(1-Elteq!$F$6)","v":2.0624485321649022}]
["ANAMET-S",2972260,"-","Steel fittings for Sealtite, Ferrule, galvanised steel",25,3.0007697112128979,{"$f":"F1932*(1-Elteq!$F$6)","v":3.0007697112128979}]
["ANAMET-S",2972350,"-","Steel fittings for Sealtite, Ferrule, galvanised steel",5,7.0234733798048001,{"$f":"F1933*(1-Elteq!$F$6)","v":7.0234733798048001}]
["ANAMET-S",2972400,"-","Steel fittings for Sealtite, Ferrule, galvanised steel",5,9.0208897510455852,{"$f":"F1934*(1-Elteq!$F$6)","v":9.0208897510455852}]
["ANAMET-S",2972500,"-","Steel fittings for Sealtite, Ferrule, galvanised steel",5,12.532626440947986,{"$f":"F1935*(1-Elteq!$F$6)","v":12.532626440947986}]
["ANAMET-S",2972630,"-","Steel fittings for Sealtite, Ferrule, galvanised steel",25,52.945469300935933,{"$f":"F1936*(1-Elteq!$F$6)","v":52.945469300935933}]
["ANAMET-S",2972750,"-","Steel fittings for Sealtite, Ferrule, galvanised steel",25,71.544667325233831,{"$f":"F1937*(1-Elteq!$F$6)","v":71.544667325233831}]
["ANAMET-S",2972990,"-","Steel fittings for Sealtite, Ferrule, galvanised steel",1,124.21142736506637,{"$f":"F1938*(1-Elteq!$F$6)","v":124.21142736506637}]
["ANAMET-S",2974160,"-","Steel fittings for Sealtite, Locknut, galvanised steel",100,0.4273542003584932,{"$f":"F1939*(1-Elteq!$F$6)","v":0.4273542003584932}]
["ANAMET-S",2974200,"-","Steel fittings for Sealtite, Locknut, galvanised steel",100,0.71535377016530377,{"$f":"F1940*(1-Elteq!$F$6)","v":0.71535377016530377}]
["ANAMET-S",2974260,"-","Steel fittings for Sealtite, Locknut, galvanised steel",50,1.235611057558252,{"$f":"F1941*(1-Elteq!$F$6)","v":1.235611057558252}]
["ANAMET-S",2974350,"-","Steel fittings for Sealtite, Locknut, galvanised steel",50,1.4864493925512807,{"$f":"F1942*(1-Elteq!$F$6)","v":1.4864493925512807}]
["ANAMET-S",2974400,"-","Steel fittings for Sealtite, Locknut, galvanised steel",50,2.2668353236407031,{"$f":"F1943*(1-Elteq!$F$6)","v":2.2668353236407031}]
["ANAMET-S",2974500,"-","Steel fittings for Sealtite, Locknut, galvanised steel",25,3.4002529854610546,{"$f":"F1944*(1-Elteq!$F$6)","v":3.4002529854610546}]
["ANAMET-S",2974630,"-","Steel fittings for Sealtite, Locknut, galvanised steel",1,8.8072126508663384,{"$f":"F1945*(1-Elteq!$F$6)","v":8.8072126508663384}]
["ANAMET-S",2974750,"-","Steel fittings for Sealtite, Locknut, galvanised steel",1,11.25985414857595,{"$f":"F1946*(1-Elteq!$F$6)","v":11.25985414857595}]
["ANAMET-S",2974990,"-","Steel fittings for Sealtite, Locknut, galvanised steel",1,23.829641824337717,{"$f":"F1947*(1-Elteq!$F$6)","v":23.829641824337717}]
["ANAMET-S",2982120,"22/25 mm","Steel fittings for Sealtite, Straight box connector, IP 67",25,10.349403895638291,{"$f":"F1948*(1-Elteq!$F$6)","v":10.349403895638291}]
["ANAMET-S",2982160,"22/25 mm","Steel fittings for Sealtite, Straight box connector, IP 67",25,10.349403895638291,{"$f":"F1949*(1-Elteq!$F$6)","v":10.349403895638291}]
["ANAMET-S",2982200,"28/31 mm","Steel fittings for Sealtite, Straight box connector, IP 67",25,14.660107134037005,{"$f":"F1950*(1-Elteq!$F$6)","v":14.660107134037005}]
["ANAMET-S",2982260,"34/37 mm","Steel fittings for Sealtite, Straight box connector, IP 67",5,22.779836940848373,{"$f":"F1951*(1-Elteq!$F$6)","v":22.779836940848373}]
["ANAMET-S",2982350,"43/47 mm","Steel fittings for Sealtite, Straight box connector, IP 67",5,35.488979247161829,{"$f":"F1952*(1-Elteq!$F$6)","v":35.488979247161829}]
["ANAMET-S",2982400,"49/53 mm","Steel fittings for Sealtite, Straight box connector, IP 67",2,56.327141668990095,{"$f":"F1953*(1-Elteq!$F$6)","v":56.327141668990095}]
["ANAMET-S",2982500,"61/66 mm","Steel fittings for Sealtite, Straight box connector, IP 67",1,79.469300649272853,{"$f":"F1954*(1-Elteq!$F$6)","v":79.469300649272853}]
["ANAMET-S",2988120,"22/25 mm","Steel fittings for Sealtite, 90° elbow box connector, IP 67",25,18.088231045608396,{"$f":"F1955*(1-Elteq!$F$6)","v":18.088231045608396}]
["ANAMET-S",2988160,"22/25 mm","Steel fittings for Sealtite, 90° elbow box connector, IP 67",25,18.088231045608396,{"$f":"F1956*(1-Elteq!$F$6)","v":18.088231045608396}]
["ANAMET-S",2988200,"28/31 mm","Steel fittings for Sealtite, 90° elbow box connector, IP 67",10,28.725634511053499,{"$f":"F1957*(1-Elteq!$F$6)","v":28.725634511053499}]
["ANAMET-S",2988260,"34/37 mm","Steel fittings for Sealtite, 90° elbow box connector, IP 67",5,38.731296984664304,{"$f":"F1958*(1-Elteq!$F$6)","v":38.731296984664304}]
["ANAMET-S",2989120,"NPT 1/2\"","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",25,10.823209639514012,{"$f":"F1959*(1-Elteq!$F$6)","v":10.823209639514012}]
["ANAMET-S",2989160,"NPT 1/2\"","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",25,10.823209639514012,{"$f":"F1960*(1-Elteq!$F$6)","v":10.823209639514012}]
["ANAMET-S",2989200,"NPT 3/4\"","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",25,16.369523935470976,{"$f":"F1961*(1-Elteq!$F$6)","v":16.369523935470976}]
["ANAMET-S",2989260,"NPT 1\"","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",5,31.011050452101095,{"$f":"F1962*(1-Elteq!$F$6)","v":31.011050452101095}]
["ANAMET-S",2989350,"NPT 1 1/4\"","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",5,50.232699159529837,{"$f":"F1963*(1-Elteq!$F$6)","v":50.232699159529837}]
["ANAMET-S",2989400,"NPT 1 1/2\"","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",2,61.046618490340407,{"$f":"F1964*(1-Elteq!$F$6)","v":61.046618490340407}]
["ANAMET-S",2989500,"NPT 2\"","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,95.262825445130204,{"$f":"F1965*(1-Elteq!$F$6)","v":95.262825445130204}]
["ANAMET-S",2989630,"NPT 2 1/2\"","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,480.2717987333188,{"$f":"F1966*(1-Elteq!$F$6)","v":480.2717987333188}]
["ANAMET-S",2989750,"NPT 3\"","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,545.70344293168546,{"$f":"F1967*(1-Elteq!$F$6)","v":545.70344293168546}]
["ANAMET-S",2989990,"NPT 4\"","Steel fittings for Sealtite, 90° elbow fixed with male thread, IP 67",1,673.24080081258535,{"$f":"F1968*(1-Elteq!$F$6)","v":673.24080081258535}]
["ANAMET-S",8103032,"PG11","Special fittings for Sealtite, Power connector adapter, IP 67",10,10.154307412865935,{"$f":"F1969*(1-Elteq!$F$6)","v":10.154307412865935}]
["ANAMET-S",8103036,"PG11","Special fittings for Sealtite, Power connector adapter, IP 67",10,10.897532109141576,{"$f":"F1970*(1-Elteq!$F$6)","v":10.897532109141576}]
["ANAMET-S",8103037,"PG11","Special fittings for Sealtite, Power connector adapter, IP 67",10,12.662690762796222,{"$f":"F1971*(1-Elteq!$F$6)","v":12.662690762796222}]
["ANAMET-S",8103041,"PG11","Special fittings for Sealtite, Power connector adapter, IP 67",10,8.9651478988249114,{"$f":"F1972*(1-Elteq!$F$6)","v":8.9651478988249114}]
["ANAMET-S",8103045,"PG11","Special fittings for Sealtite, Power connector adapter, IP 68",10,11.101918900617378,{"$f":"F1973*(1-Elteq!$F$6)","v":11.101918900617378}]
["ANAMET-S",8103046,"PG11","Special fittings for Sealtite, Power connector adapter, IP 40",10,11.845143596893019,{"$f":"F1974*(1-Elteq!$F$6)","v":11.845143596893019}]
["ANAMET-S",8103047,"PG11","Special fittings for Sealtite, Power connector adapter, IP 40",10,11.287725074686287,{"$f":"F1975*(1-Elteq!$F$6)","v":11.287725074686287}]
["ANAMET-S",8123231,"M24 x 1","Special fittings for Sealtite, Power connector adapter, IP 67",10,8.9651478988249114,{"$f":"F1976*(1-Elteq!$F$6)","v":8.9651478988249114}]
["ANAMET-S",8123235,"M24 x 1","Special fittings for Sealtite, Power connector adapter, IP 68",10,11.101918900617378,{"$f":"F1977*(1-Elteq!$F$6)","v":11.101918900617378}]
["ANAMET-S",8123236,"M24 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",10,11.845143596893019,{"$f":"F1978*(1-Elteq!$F$6)","v":11.845143596893019}]
["ANAMET-S",8123237,"M24 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",10,11.287725074686287,{"$f":"F1979*(1-Elteq!$F$6)","v":11.287725074686287}]
["ANAMET-S",8123271,"M25 x 1","Special fittings for Sealtite, Power connector adapter, IP 67",10,10.981144887472585,{"$f":"F1980*(1-Elteq!$F$6)","v":10.981144887472585}]
["ANAMET-S",8123275,"M25 x 1","Special fittings for Sealtite, Power connector adapter, IP 68",10,13.303722063333963,{"$f":"F1981*(1-Elteq!$F$6)","v":13.303722063333963}]
["ANAMET-S",8123276,"M25 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",10,13.861140585540692,{"$f":"F1982*(1-Elteq!$F$6)","v":13.861140585540692}]
["ANAMET-S",8123277,"M25 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",10,14.000495216092375,{"$f":"F1983*(1-Elteq!$F$6)","v":14.000495216092375}]
["ANAMET-S",8123291,"M25 x 1","Special fittings for Sealtite, Power connector adapter, IP 67",5,12.727722923720341,{"$f":"F1984*(1-Elteq!$F$6)","v":12.727722923720341}]
["ANAMET-S",8123295,"M25 x 1","Special fittings for Sealtite, Power connector adapter, IP 68",5,15.050300099581717,{"$f":"F1985*(1-Elteq!$F$6)","v":15.050300099581717}]
["ANAMET-S",8123296,"M25 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",5,16.44384640509854,{"$f":"F1986*(1-Elteq!$F$6)","v":16.44384640509854}]
["ANAMET-S",8123297,"M25 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",5,17.279974188408641,{"$f":"F1987*(1-Elteq!$F$6)","v":17.279974188408641}]
["ANAMET-S",8123381,"M40 x 1","Special fittings for Sealtite, Power connector adapter, IP 67",5,19.203068090021858,{"$f":"F1988*(1-Elteq!$F$6)","v":19.203068090021858}]
["ANAMET-S",8123386,"M40 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",5,24.870156399123612,{"$f":"F1989*(1-Elteq!$F$6)","v":24.870156399123612}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8123387,"M40 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",5,27.099830487950538,{"$f":"F1990*(1-Elteq!$F$6)","v":27.099830487950538}]
["ANAMET-S",8123421,"M40 x 1","Special fittings for Sealtite, Power connector adapter, IP 67",2,41.722776387173759,{"$f":"F1991*(1-Elteq!$F$6)","v":41.722776387173759}]
["ANAMET-S",8123426,"M40 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",2,45.253093694483056,{"$f":"F1992*(1-Elteq!$F$6)","v":45.253093694483056}]
["ANAMET-S",8123427,"M40 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",2,50.176957307309166,{"$f":"F1993*(1-Elteq!$F$6)","v":50.176957307309166}]
["ANAMET-S",8175120,"13 mm","Special fittings for Sealtite, Clamping ring for mounting fittings",10,1.6722555666201908,{"$f":"F1994*(1-Elteq!$F$6)","v":1.6722555666201908}]
["ANAMET-S",8175160,"16 mm","Special fittings for Sealtite, Clamping ring for mounting fittings",10,2.1367710017924657,{"$f":"F1995*(1-Elteq!$F$6)","v":2.1367710017924657}]
["ANAMET-S",8175200,"22 mm","Special fittings for Sealtite, Clamping ring for mounting fittings",5,2.5548348934475134,{"$f":"F1996*(1-Elteq!$F$6)","v":2.5548348934475134}]
["ANAMET-S",8175260,"25 mm","Special fittings for Sealtite, Clamping ring for mounting fittings",5,3.3909626767576091,{"$f":"F1997*(1-Elteq!$F$6)","v":3.3909626767576091}]
["ANAMET-S",8175350,"35 mm","Special fittings for Sealtite, Clamping ring for mounting fittings",2,3.9483811989643396,{"$f":"F1998*(1-Elteq!$F$6)","v":3.9483811989643396}]
["ANAMET-S",8175400,"38 mm","Special fittings for Sealtite, Clamping ring for mounting fittings",2,6.7819253535152182,{"$f":"F1999*(1-Elteq!$F$6)","v":6.7819253535152182}]
["ANAMET-S",8175500,"51 mm","Special fittings for Sealtite, Clamping ring for mounting fittings",2,12.449013662616975,{"$f":"F2000*(1-Elteq!$F$6)","v":12.449013662616975}]
["ANAMET-S",8123221,"M25 x 1","Special fittings for Sealtite, Power connector adapter, IP 67",10,8.9651478988249114,{"$f":"F2001*(1-Elteq!$F$6)","v":8.9651478988249114}]
["ANAMET-S",8123226,"M25 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",10,11.845143596893019,{"$f":"F2002*(1-Elteq!$F$6)","v":11.845143596893019}]
["ANAMET-S",8123227,"M25 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",10,11.287725074686287,{"$f":"F2003*(1-Elteq!$F$6)","v":11.287725074686287}]
["ANAMET-S",8123261,"M24 x 1","Special fittings for Sealtite, Power connector adapter, IP 67",10,8.9651478988249114,{"$f":"F2004*(1-Elteq!$F$6)","v":8.9651478988249114}]
["ANAMET-S",8123266,"M24 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",10,11.845143596893019,{"$f":"F2005*(1-Elteq!$F$6)","v":11.845143596893019}]
["ANAMET-S",8123267,"M24 x 1","Special fittings for Sealtite, Power connector adapter, IP 40",10,11.984498227444702,{"$f":"F2006*(1-Elteq!$F$6)","v":11.984498227444702}]
["ANAMET-S",8833080,"M8 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 65",10,13.823979350726912,{"$f":"F2007*(1-Elteq!$F$6)","v":13.823979350726912}]
["ANAMET-S",8833086,"M8 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",10,14.56720404700255,{"$f":"F2008*(1-Elteq!$F$6)","v":14.56720404700255}]
["ANAMET-S",8833087,"M8 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",10,14.56720404700255,{"$f":"F2009*(1-Elteq!$F$6)","v":14.56720404700255}]
["ANAMET-S",8833100,"M8 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 65",10,13.823979350726912,{"$f":"F2010*(1-Elteq!$F$6)","v":13.823979350726912}]
["ANAMET-S",8833106,"M8 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",10,14.56720404700255,{"$f":"F2011*(1-Elteq!$F$6)","v":14.56720404700255}]
["ANAMET-S",8833107,"M8 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",10,16.146556526588284,{"$f":"F2012*(1-Elteq!$F$6)","v":16.146556526588284}]
["ANAMET-S",8833120,"M12 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 65",10,13.823979350726912,{"$f":"F2013*(1-Elteq!$F$6)","v":13.823979350726912}]
["ANAMET-S",8833126,"M12 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",10,14.56720404700255,{"$f":"F2014*(1-Elteq!$F$6)","v":14.56720404700255}]
["ANAMET-S",8833127,"M12 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",10,14.56720404700255,{"$f":"F2015*(1-Elteq!$F$6)","v":14.56720404700255}]
["ANAMET-S",8833140,"M18 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 65",10,12.755593849830678,{"$f":"F2016*(1-Elteq!$F$6)","v":12.755593849830678}]
["ANAMET-S",8833146,"M18 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",10,13.498818546106316,{"$f":"F2017*(1-Elteq!$F$6)","v":13.498818546106316}]
["ANAMET-S",8833147,"M18 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",10,13.498818546106316,{"$f":"F2018*(1-Elteq!$F$6)","v":13.498818546106316}]
["ANAMET-S",8833160,"M12 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 65",10,13.823979350726912,{"$f":"F2019*(1-Elteq!$F$6)","v":13.823979350726912}]
["ANAMET-S",8833166,"M12 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",10,14.56720404700255,{"$f":"F2020*(1-Elteq!$F$6)","v":14.56720404700255}]
["ANAMET-S",8833167,"M12 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",10,16.146556526588284,{"$f":"F2021*(1-Elteq!$F$6)","v":16.146556526588284}]
["ANAMET-S",8833180,"M18 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 65",10,12.755593849830678,{"$f":"F2022*(1-Elteq!$F$6)","v":12.755593849830678}]
["ANAMET-S",8833186,"M18 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",10,13.498818546106316,{"$f":"F2023*(1-Elteq!$F$6)","v":13.498818546106316}]
["ANAMET-S",8833187,"M18 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 40",10,15.263977199760962,{"$f":"F2024*(1-Elteq!$F$6)","v":15.263977199760962}]
["ANAMET-S",8150060,"1/4\"","Fitting accessories for Sealtite, Ferrule, nickel plated brass",10,2.0252872973511198,{"$f":"F2025*(1-Elteq!$F$6)","v":2.0252872973511198}]
["ANAMET-S",8150100,"5/16\"","Fitting accessories for Sealtite, Ferrule, nickel plated brass",10,2.0252872973511198,{"$f":"F2026*(1-Elteq!$F$6)","v":2.0252872973511198}]
["ANAMET-S",8150110,"3/8\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",10,0.91974056164110485,{"$f":"F2027*(1-Elteq!$F$6)","v":0.91974056164110485}]
["ANAMET-S",8150112,"3/8\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",50,0.73393438757219487,{"$f":"F2028*(1-Elteq!$F$6)","v":0.73393438757219487}]
["ANAMET-S",8150113,"3/8\"","Fitting accessories for Sealtite, Ferrule, nickel plated brass",10,2.303996558454485,{"$f":"F2029*(1-Elteq!$F$6)","v":2.303996558454485}]
["ANAMET-S",8150117,"3/8\"","Fitting accessories for Sealtite, Ferrule, plastic (POM)",10,1.727997418840864,{"$f":"F2030*(1-Elteq!$F$6)","v":1.727997418840864}]
["ANAMET-S",8150160,"1/2\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",10,0.97548241386177792,{"$f":"F2031*(1-Elteq!$F$6)","v":0.97548241386177792}]
["ANAMET-S",8150162,"1/2\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",50,0.78038593108942222,{"$f":"F2032*(1-Elteq!$F$6)","v":0.78038593108942222}]
["ANAMET-S",8150163,"1/2\"","Fitting accessories for Sealtite, Ferrule, nickel plated brass",10,2.7778023023302061,{"$f":"F2033*(1-Elteq!$F$6)","v":2.7778023023302061}]
["ANAMET-S",8150167,"1/2\"","Fitting accessories for Sealtite, Ferrule, plastic (POM)",10,2.0810291495717932,{"$f":"F2034*(1-Elteq!$F$6)","v":2.0810291495717932}]
["ANAMET-S",8150210,"3/4\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",5,1.0405145747858966,{"$f":"F2035*(1-Elteq!$F$6)","v":1.0405145747858966}]
["ANAMET-S",8150212,"3/4\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",25,0.83612778331009541,{"$f":"F2036*(1-Elteq!$F$6)","v":0.83612778331009541}]
["ANAMET-S",8150213,"3/4\"","Fitting accessories for Sealtite, Ferrule, nickel plated brass",5,3.3073498984265992,{"$f":"F2037*(1-Elteq!$F$6)","v":3.3073498984265992}]
["ANAMET-S",8150217,"3/4\"","Fitting accessories for Sealtite, Ferrule, plastic (POM)",10,2.4805124238199494,{"$f":"F2038*(1-Elteq!$F$6)","v":2.4805124238199494}]
["ANAMET-S",8150290,"1\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",2,1.1148370444134605,{"$f":"F2039*(1-Elteq!$F$6)","v":1.1148370444134605}]
["ANAMET-S",8150292,"1\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",25,0.89186963553076837,{"$f":"F2040*(1-Elteq!$F$6)","v":0.89186963553076837}]
["ANAMET-S",8150293,"1\"","Fitting accessories for Sealtite, Ferrule, nickel plated brass",5,4.4314772515435052,{"$f":"F2041*(1-Elteq!$F$6)","v":4.4314772515435052}]
["ANAMET-S",8150297,"1\"","Fitting accessories for Sealtite, Ferrule, plastic (POM)",10,3.3259305158334906,{"$f":"F2042*(1-Elteq!$F$6)","v":3.3259305158334906}]
["ANAMET-S",8150362,"1.1/4\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",10,1.3470947619995981,{"$f":"F2043*(1-Elteq!$F$6)","v":1.3470947619995981}]
["ANAMET-S",8150363,"1 1/4\"","Fitting accessories for Sealtite, Ferrule, nickel plated brass",2,5.815733248356886,{"$f":"F2044*(1-Elteq!$F$6)","v":5.815733248356886}]
["ANAMET-S",8150367,"1 1/4\"","Fitting accessories for Sealtite, Ferrule, plastic (POM)",10,4.3664450906193863,{"$f":"F2045*(1-Elteq!$F$6)","v":4.3664450906193863}]
["ANAMET-S",8150422,"1 1/2\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",10,1.7930295797649822,{"$f":"F2046*(1-Elteq!$F$6)","v":1.7930295797649822}]
["ANAMET-S",8150423,"1 1/2\"","Fitting accessories for Sealtite, Ferrule, nickel plated brass",2,8.0268267197769152,{"$f":"F2047*(1-Elteq!$F$6)","v":8.0268267197769152}]
["ANAMET-S",8150482,"2\"","Fitting accessories for Sealtite, Ferrule, galvanised steel",10,2.8149635371439876,{"$f":"F2048*(1-Elteq!$F$6)","v":2.8149635371439876}]
["ANAMET-S",8150483,"2\"","Fitting accessories for Sealtite, Ferrule, nickel plated brass",2,12.049530388368819,{"$f":"F2049*(1-Elteq!$F$6)","v":12.049530388368819}]
["ANAMET-S",8154160,"M 16","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,0.34374142202748365,{"$f":"F2050*(1-Elteq!$F$6)","v":0.34374142202748365}]
["ANAMET-S",8832080,"M8 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 65",25,13.582431324437325,{"$f":"F2051*(1-Elteq!$F$6)","v":13.582431324437325}]
["ANAMET-S",8832120,"M12 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 65",25,13.582431324437325,{"$f":"F2052*(1-Elteq!$F$6)","v":13.582431324437325}]
["ANAMET-S",8832180,"M18 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 65",25,15.35688028679542,{"$f":"F2053*(1-Elteq!$F$6)","v":15.35688028679542}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8832300,"M30 x 1,5","Special fittings for Sealtite, Proximity switch adapter, IP 65",25,22.222418418641649,{"$f":"F2054*(1-Elteq!$F$6)","v":22.222418418641649}]
["ANAMET-S",8833200,"I.D. 20 mm","Special fittings for Sealtite, Proximity switch adapter, IP 65",25,23.374416697868892,{"$f":"F2055*(1-Elteq!$F$6)","v":23.374416697868892}]
["ANAMET-S",8833340,"I.D. 34 mm","Special fittings for Sealtite, Proximity switch adapter, IP 65",25,31.967952248555974,{"$f":"F2056*(1-Elteq!$F$6)","v":31.967952248555974}]
["ANAMET-S",8840080,"M8 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 67",10,14.399978490340532,{"$f":"F2057*(1-Elteq!$F$6)","v":14.399978490340532}]
["ANAMET-S",8840120,"M12 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 67",10,14.399978490340532,{"$f":"F2058*(1-Elteq!$F$6)","v":14.399978490340532}]
["ANAMET-S",8840140,"M14 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 67",10,14.399978490340532,{"$f":"F2059*(1-Elteq!$F$6)","v":14.399978490340532}]
["ANAMET-S",8840180,"M18 x 1","Special fittings for Sealtite, Proximity switch adapter, IP 67",10,14.399978490340532,{"$f":"F2060*(1-Elteq!$F$6)","v":14.399978490340532}]
["ANAMET-S",8840300,"M30 x 1,5","Special fittings for Sealtite, Proximity switch adapter, IP 67",5,20.20642142999397,{"$f":"F2061*(1-Elteq!$F$6)","v":20.20642142999397}]
["ANAMET-S",8154200,"M 20","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,0.37161234813782018,{"$f":"F2062*(1-Elteq!$F$6)","v":0.37161234813782018}]
["ANAMET-S",8154250,"M 25","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,0.39019296554471111,{"$f":"F2063*(1-Elteq!$F$6)","v":0.39019296554471111}]
["ANAMET-S",8154320,"M 32","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,0.39948327424815672,{"$f":"F2064*(1-Elteq!$F$6)","v":0.39948327424815672}]
["ANAMET-S",8154400,"M 40","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,0.60387006572395774,{"$f":"F2065*(1-Elteq!$F$6)","v":0.60387006572395774}]
["ANAMET-S",8154500,"M 50","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,0.92903087034455045,{"$f":"F2066*(1-Elteq!$F$6)","v":0.92903087034455045}]
["ANAMET-S",8154630,"M 63","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,1.3470947619995981,{"$f":"F2067*(1-Elteq!$F$6)","v":1.3470947619995981}]
["ANAMET-S",8155070,"PG 7 / - / -","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,0.3344511133240381,{"$f":"F2068*(1-Elteq!$F$6)","v":0.3344511133240381}]
["ANAMET-S",8155090,"PG 9 / M16/ -","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,0.3344511133240381,{"$f":"F2069*(1-Elteq!$F$6)","v":0.3344511133240381}]
["ANAMET-S",8155110,"PG 11 / - / -","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,0.34374142202748365,{"$f":"F2070*(1-Elteq!$F$6)","v":0.34374142202748365}]
["ANAMET-S",8155130,"PG 13,5 / - / -","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,0.36232203943437469,{"$f":"F2071*(1-Elteq!$F$6)","v":0.36232203943437469}]
["ANAMET-S",8155160,"PG 16 / - / 1/2\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",100,0.37161234813782018,{"$f":"F2072*(1-Elteq!$F$6)","v":0.37161234813782018}]
["ANAMET-S",8155210,"PG 21 /  - / 3/4\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",50,0.39019296554471111,{"$f":"F2073*(1-Elteq!$F$6)","v":0.39019296554471111}]
["ANAMET-S",8155290,"PG 29 / - / 1\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",50,0.39948327424815672,{"$f":"F2074*(1-Elteq!$F$6)","v":0.39948327424815672}]
["ANAMET-S",8155360,"PG 36 / - / 1 1/4\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",50,0.60387006572395774,{"$f":"F2075*(1-Elteq!$F$6)","v":0.60387006572395774}]
["ANAMET-S",8155420,"PG 42 / - / 1 1/2\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",50,0.92903087034455045,{"$f":"F2076*(1-Elteq!$F$6)","v":0.92903087034455045}]
["ANAMET-S",8155480,"PG 48 / - / 2\"","Fitting accessories for Sealtite, Seal ring flat, neoprene",50,1.3470947619995981,{"$f":"F2077*(1-Elteq!$F$6)","v":1.3470947619995981}]
["ANAMET-S",8156160,"NPT 1/2\"","Fitting accessories for Sealtite, Seal ring round, NBR",100,5.5741852220673023E-2,{"$f":"F2078*(1-Elteq!$F$6)","v":5.5741852220673023E-2}]
["ANAMET-S",8156200,"NPT 3/4\"","Fitting accessories for Sealtite, Seal ring round, NBR",50,7.4322469627564031E-2,{"$f":"F2079*(1-Elteq!$F$6)","v":7.4322469627564031E-2}]
["ANAMET-S",8156260,"NPT 1\"","Fitting accessories for Sealtite, Seal ring round, NBR",50,8.3612778331009524E-2,{"$f":"F2080*(1-Elteq!$F$6)","v":8.3612778331009524E-2}]
["ANAMET-S",8156350,"NPT 1.1/4\"","Fitting accessories for Sealtite, Seal ring round, NBR",20,0.11148370444134605,{"$f":"F2081*(1-Elteq!$F$6)","v":0.11148370444134605}]
["ANAMET-S",8156400,"NPT 1.1/2\"","Fitting accessories for Sealtite, Seal ring round, NBR",20,0.13006432184823707,{"$f":"F2082*(1-Elteq!$F$6)","v":0.13006432184823707}]
["ANAMET-S",8156500,"NPT 2\"","Fitting accessories for Sealtite, Seal ring round, NBR",20,0.15793524795857358,{"$f":"F2083*(1-Elteq!$F$6)","v":0.15793524795857358}]
["ANAMET-S",8800070," PG 7","Fitting accessories for Sealtite, Locknut, nickel plated brass",50,0.15793524795857358,{"$f":"F2084*(1-Elteq!$F$6)","v":0.15793524795857358}]
["ANAMET-S",8800090,"PG 9","Fitting accessories for Sealtite, Locknut, nickel plated brass",50,0.15793524795857358,{"$f":"F2085*(1-Elteq!$F$6)","v":0.15793524795857358}]
["ANAMET-S",8800110,"PG 11","Fitting accessories for Sealtite, Locknut, nickel plated brass",50,0.1765158653654646,{"$f":"F2086*(1-Elteq!$F$6)","v":0.1765158653654646}]
["ANAMET-S",8800130,"PG 13,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",50,0.1765158653654646,{"$f":"F2087*(1-Elteq!$F$6)","v":0.1765158653654646}]
["ANAMET-S",8800160,"PG 16","Fitting accessories for Sealtite, Locknut, nickel plated brass",50,0.22296740888269209,{"$f":"F2088*(1-Elteq!$F$6)","v":0.22296740888269209}]
["ANAMET-S",8800210,"PG 21","Fitting accessories for Sealtite, Locknut, nickel plated brass",20,0.34374142202748365,{"$f":"F2089*(1-Elteq!$F$6)","v":0.34374142202748365}]
["ANAMET-S",8800290,"PG 29","Fitting accessories for Sealtite, Locknut, nickel plated brass",20,0.53883790479983917,{"$f":"F2090*(1-Elteq!$F$6)","v":0.53883790479983917}]
["ANAMET-S",8800360,"PG 36","Fitting accessories for Sealtite, Locknut, nickel plated brass",10,1.3006432184823704,{"$f":"F2091*(1-Elteq!$F$6)","v":1.3006432184823704}]
["ANAMET-S",8800420,"PG 42","Fitting accessories for Sealtite, Locknut, nickel plated brass",5,2.0624485321649022,{"$f":"F2092*(1-Elteq!$F$6)","v":2.0624485321649022}]
["ANAMET-S",8800480,"PG 48","Fitting accessories for Sealtite, Locknut, nickel plated brass",5,2.0996097669786837,{"$f":"F2093*(1-Elteq!$F$6)","v":2.0996097669786837}]
["ANAMET-S",8801120,"M12x1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",50,0.15793524795857358,{"$f":"F2094*(1-Elteq!$F$6)","v":0.15793524795857358}]
["ANAMET-S",8801160,"M16 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",50,0.20438679147580111,{"$f":"F2095*(1-Elteq!$F$6)","v":0.20438679147580111}]
["ANAMET-S",8801200,"M20 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",50,0.27870926110336514,{"$f":"F2096*(1-Elteq!$F$6)","v":0.27870926110336514}]
["ANAMET-S",8801250,"M25 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",25,0.39948327424815672,{"$f":"F2097*(1-Elteq!$F$6)","v":0.39948327424815672}]
["ANAMET-S",8801320,"M32 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",20,0.5016766699860572,{"$f":"F2098*(1-Elteq!$F$6)","v":0.5016766699860572}]
["ANAMET-S",8801400,"M40 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",10,1.2449013662616977,{"$f":"F2099*(1-Elteq!$F$6)","v":1.2449013662616977}]
["ANAMET-S",8801500,"M50 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",10,2.0067066799442288,{"$f":"F2100*(1-Elteq!$F$6)","v":2.0067066799442288}]
["ANAMET-S",8801630,"M63 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",5,2.8242538458474336,{"$f":"F2101*(1-Elteq!$F$6)","v":2.8242538458474336}]
["ANAMET-S",8802160,"NPT 1/2\"","Fitting accessories for Sealtite, Locknut, nickel plated brass",50,0.5202572873929483,{"$f":"F2102*(1-Elteq!$F$6)","v":0.5202572873929483}]
["ANAMET-S",8802200,"NPT 3/4\"","Fitting accessories for Sealtite, Locknut, nickel plated brass",20,0.65961191794463081,{"$f":"F2103*(1-Elteq!$F$6)","v":0.65961191794463081}]
["ANAMET-S",8802260,"NPT 1 \"","Fitting accessories for Sealtite, Locknut, nickel plated brass",20,1.124127353116906,{"$f":"F2104*(1-Elteq!$F$6)","v":1.124127353116906}]
["ANAMET-S",8802350,"NPT 1 1/4\"","Fitting accessories for Sealtite, Locknut, nickel plated brass",25,1.6350943318064088,{"$f":"F2105*(1-Elteq!$F$6)","v":1.6350943318064088}]
["ANAMET-S",8802400,"NPT 1 1/2\"","Fitting accessories for Sealtite, Locknut, nickel plated brass",10,2.8799956980681065,{"$f":"F2106*(1-Elteq!$F$6)","v":2.8799956980681065}]
["ANAMET-S",8802500,"NPT 2\"","Fitting accessories for Sealtite, Locknut, nickel plated brass",10,5.6020561481776392,{"$f":"F2107*(1-Elteq!$F$6)","v":5.6020561481776392}]
["ANAMET-S",8803160,"NPT 1/2\"","Fitting accessories for Sealtite, Locknut, galvanised steel",100,0.28799956980681063,{"$f":"F2108*(1-Elteq!$F$6)","v":0.28799956980681063}]
["ANAMET-S",8803200,"NPT 3/4\"","Fitting accessories for Sealtite, Locknut, galvanised steel",50,0.48309605257916621,{"$f":"F2109*(1-Elteq!$F$6)","v":0.48309605257916621}]
["ANAMET-S",8803260,"NPT 1 \"","Fitting accessories for Sealtite, Locknut, galvanised steel",50,0.57599913961362126,{"$f":"F2110*(1-Elteq!$F$6)","v":0.57599913961362126}]
["ANAMET-S",8803350,"NPT 1 1/4\"","Fitting accessories for Sealtite, Locknut, galvanised steel",20,1.0126436486755599,{"$f":"F2111*(1-Elteq!$F$6)","v":1.0126436486755599}]
["ANAMET-S",8803400,"NPT 1 1/2\"","Fitting accessories for Sealtite, Locknut, galvanised steel",20,1.2727722923720342,{"$f":"F2112*(1-Elteq!$F$6)","v":1.2727722923720342}]
["ANAMET-S",8803500,"NPT 2\"","Fitting accessories for Sealtite, Locknut, galvanised steel",20,1.8394811232822097,{"$f":"F2113*(1-Elteq!$F$6)","v":1.8394811232822097}]
["ANAMET-S",8810070,"PG 9","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",100,0.62245068313084884,{"$f":"F2114*(1-Elteq!$F$6)","v":0.62245068313084884}]
["ANAMET-S",8810080,"PG 11","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",100,0.69677315275841278,{"$f":"F2115*(1-Elteq!$F$6)","v":0.69677315275841278}]
["ANAMET-S",8810090,"PG 11","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",100,0.69677315275841278,{"$f":"F2116*(1-Elteq!$F$6)","v":0.69677315275841278}]
["ANAMET-S",8810110,"PG 13,5","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",100,0.70606346146185839,{"$f":"F2117*(1-Elteq!$F$6)","v":0.70606346146185839}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8810120,"PG 16","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",100,0.97548241386177792,{"$f":"F2118*(1-Elteq!$F$6)","v":0.97548241386177792}]
["ANAMET-S",8810130,"PG 16","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",100,0.77109562238597684,{"$f":"F2119*(1-Elteq!$F$6)","v":0.77109562238597684}]
["ANAMET-S",8810150,"PG 21","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",50,1.8673520493925462,{"$f":"F2120*(1-Elteq!$F$6)","v":1.8673520493925462}]
["ANAMET-S",8810160,"PG 21","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",50,1.6908361840270818,{"$f":"F2121*(1-Elteq!$F$6)","v":1.6908361840270818}]
["ANAMET-S",8810210,"PG 29","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",25,2.9728987851025614,{"$f":"F2122*(1-Elteq!$F$6)","v":2.9728987851025614}]
["ANAMET-S",8810290,"PG 36","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",25,6.0387006572395778,{"$f":"F2123*(1-Elteq!$F$6)","v":6.0387006572395778}]
["ANAMET-S",8810360,"PG 42","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",25,11.993788536148145,{"$f":"F2124*(1-Elteq!$F$6)","v":11.993788536148145}]
["ANAMET-S",8810420,"PG 48","Fitting accessories for Sealtite, Reducer PG/PG nickel plated brass",25,15.078171025692054,{"$f":"F2125*(1-Elteq!$F$6)","v":15.078171025692054}]
["ANAMET-S",8811070,"M 12 x 1,5","Fitting accessories for Sealtite, Adapter ISO/PG nickel plated brass",100,1.8116101971718732,{"$f":"F2126*(1-Elteq!$F$6)","v":1.8116101971718732}]
["ANAMET-S",8811090,"M 16 X 1,5","Fitting accessories for Sealtite, Adapter ISO/PG nickel plated brass",50,2.0996097669786837,{"$f":"F2127*(1-Elteq!$F$6)","v":2.0996097669786837}]
["ANAMET-S",8811110,"M 20 X 1,5","Fitting accessories for Sealtite, Adapter ISO/PG nickel plated brass",50,2.6756089065923048,{"$f":"F2128*(1-Elteq!$F$6)","v":2.6756089065923048}]
["ANAMET-S",8811160,"M 25 X 1,5","Fitting accessories for Sealtite, Adapter ISO/PG nickel plated brass",50,4.3478644732124963,{"$f":"F2129*(1-Elteq!$F$6)","v":4.3478644732124963}]
["ANAMET-S",8811210,"M 32 X 1,5","Fitting accessories for Sealtite, Adapter ISO/PG nickel plated brass",20,7.3579244931288388,{"$f":"F2130*(1-Elteq!$F$6)","v":7.3579244931288388}]
["ANAMET-S",8811290,"M 40 X 1,5","Fitting accessories for Sealtite, Adapter ISO/PG nickel plated brass",20,9.5597276558454229,{"$f":"F2131*(1-Elteq!$F$6)","v":9.5597276558454229}]
["ANAMET-S",8811360,"M50 x 1,5","Fitting accessories for Sealtite, Adapter ISO/PG nickel plated brass",10,12.662690762796222,{"$f":"F2132*(1-Elteq!$F$6)","v":12.662690762796222}]
["ANAMET-S",8811480,"M63 x 1,5","Fitting accessories for Sealtite, Adapter ISO/PG nickel plated brass",1,83.575617096195757,{"$f":"F2133*(1-Elteq!$F$6)","v":83.575617096195757}]
["ANAMET-S",8812160,"M 12 X 1,5","Fitting accessories for Sealtite, Enlarger ISO/ISO nickel plated brass",50,1.4121269229237168,{"$f":"F2134*(1-Elteq!$F$6)","v":1.4121269229237168}]
["ANAMET-S",8812200,"M 16 X 1,5","Fitting accessories for Sealtite, Enlarger ISO/ISO nickel plated brass",50,1.4399978490340533,{"$f":"F2135*(1-Elteq!$F$6)","v":1.4399978490340533}]
["ANAMET-S",8812250,"M 20 X 1,5","Fitting accessories for Sealtite, Enlarger ISO/ISO nickel plated brass",50,2.4526414977096134,{"$f":"F2136*(1-Elteq!$F$6)","v":2.4526414977096134}]
["ANAMET-S",8812320,"M 25 X 1,5","Fitting accessories for Sealtite, Enlarger ISO/ISO nickel plated brass",20,3.8183168771161027,{"$f":"F2137*(1-Elteq!$F$6)","v":3.8183168771161027}]
["ANAMET-S",8812400,"M 32 X 1,5","Fitting accessories for Sealtite, Enlarger ISO/ISO nickel plated brass",20,5.0167666998605727,{"$f":"F2138*(1-Elteq!$F$6)","v":5.0167666998605727}]
["ANAMET-S",8812500,"M 40 X 1,5","Fitting accessories for Sealtite, Enlarger ISO/ISO nickel plated brass",10,9.8198562995418985,{"$f":"F2139*(1-Elteq!$F$6)","v":9.8198562995418985}]
["ANAMET-S",8812630,"M 50 X 1,5","Fitting accessories for Sealtite, Enlarger ISO/ISO nickel plated brass",5,13.257270519816734,{"$f":"F2140*(1-Elteq!$F$6)","v":13.257270519816734}]
["ANAMET-S",8820090,"PG 7","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",50,0.94761148775144144,{"$f":"F2141*(1-Elteq!$F$6)","v":0.94761148775144144}]
["ANAMET-S",8820110,"PG 9","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",50,0.94761148775144144,{"$f":"F2142*(1-Elteq!$F$6)","v":0.94761148775144144}]
["ANAMET-S",8820120,"PG 9","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",50,1.4399978490340533,{"$f":"F2143*(1-Elteq!$F$6)","v":1.4399978490340533}]
["ANAMET-S",8820130,"PG 11","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",50,0.96619210515833243,{"$f":"F2144*(1-Elteq!$F$6)","v":0.96619210515833243}]
["ANAMET-S",8820160,"PG 11","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",25,1.0962564270065693,{"$f":"F2145*(1-Elteq!$F$6)","v":1.0962564270065693}]
["ANAMET-S",8820170,"PG 13,5","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",25,1.9974163712407835,{"$f":"F2146*(1-Elteq!$F$6)","v":1.9974163712407835}]
["ANAMET-S",8820180,"PG 13,5","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",20,2.5362542760406228,{"$f":"F2147*(1-Elteq!$F$6)","v":2.5362542760406228}]
["ANAMET-S",8820210,"PG 16","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",20,1.9974163712407835,{"$f":"F2148*(1-Elteq!$F$6)","v":1.9974163712407835}]
["ANAMET-S",8820290,"PG 21","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",15,3.3723820593507181,{"$f":"F2149*(1-Elteq!$F$6)","v":3.3723820593507181}]
["ANAMET-S",8820360,"PG 29","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",10,6.921279984066901,{"$f":"F2150*(1-Elteq!$F$6)","v":6.921279984066901}]
["ANAMET-S",8820420,"PG 36","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",10,11.835853288189572,{"$f":"F2151*(1-Elteq!$F$6)","v":11.835853288189572}]
["ANAMET-S",8820480,"PG 42","Fitting accessories for Sealtite, Enlarger PG/PG nickel plated brass",10,12.950690332603031,{"$f":"F2152*(1-Elteq!$F$6)","v":12.950690332603031}]
["ANAMET-S",8821110,"PG 11","Fitting accessories for Sealtite, Adapter PG/ISO nickel plated brass",50,2.4247705715992764,{"$f":"F2153*(1-Elteq!$F$6)","v":2.4247705715992764}]
["ANAMET-S",8821160,"PG 16","Fitting accessories for Sealtite, Adapter PG/ISO nickel plated brass",50,4.645154351722752,{"$f":"F2154*(1-Elteq!$F$6)","v":4.645154351722752}]
["ANAMET-S",8821210,"PG 21","Fitting accessories for Sealtite, Adapter PG/ISO nickel plated brass",20,19.537519203345898,{"$f":"F2155*(1-Elteq!$F$6)","v":19.537519203345898}]
["ANAMET-S",8821290,"PG 29","Fitting accessories for Sealtite, Adapter PG/ISO nickel plated brass",20,17.214942027484522,{"$f":"F2156*(1-Elteq!$F$6)","v":17.214942027484522}]
["ANAMET-S",8821360,"PG 36","Fitting accessories for Sealtite, Adapter PG/ISO nickel plated brass",10,14.186301390161283,{"$f":"F2157*(1-Elteq!$F$6)","v":14.186301390161283}]
["ANAMET-S",8821480,"PG 48","Fitting accessories for Sealtite, Adapter PG/ISO nickel plated brass",5,20.847452730531714,{"$f":"F2158*(1-Elteq!$F$6)","v":20.847452730531714}]
["ANAMET-S",8822120,"M 16 X 1,5","Fitting accessories for Sealtite, Reducer ISO/ISO nickel plated brass",50,0.96619210515833243,{"$f":"F2159*(1-Elteq!$F$6)","v":0.96619210515833243}]
["ANAMET-S",8822160,"M 20 X 1,5","Fitting accessories for Sealtite, Reducer ISO/ISO nickel plated brass",50,1.1519982792272425,{"$f":"F2160*(1-Elteq!$F$6)","v":1.1519982792272425}]
["ANAMET-S",8822200,"M 25 X 1,5","Fitting accessories for Sealtite, Reducer ISO/ISO nickel plated brass",20,1.6722555666201908,{"$f":"F2161*(1-Elteq!$F$6)","v":1.6722555666201908}]
["ANAMET-S",8822250,"M 32 X 1,5","Fitting accessories for Sealtite, Reducer ISO/ISO nickel plated brass",20,2.6663185978888597,{"$f":"F2162*(1-Elteq!$F$6)","v":2.6663185978888597}]
["ANAMET-S",8822320,"M 40 X 1,5","Fitting accessories for Sealtite, Reducer ISO/ISO nickel plated brass",10,3.9483811989643396,{"$f":"F2163*(1-Elteq!$F$6)","v":3.9483811989643396}]
["ANAMET-S",8822400,"M 50 X 1,5","Fitting accessories for Sealtite, Reducer ISO/ISO nickel plated brass",5,8.6864386377215457,{"$f":"F2164*(1-Elteq!$F$6)","v":8.6864386377215457}]
["ANAMET-S",8822500,"M 63 X 1,5","Fitting accessories for Sealtite, Reducer ISO/ISO nickel plated brass",5,16.35094331806409,{"$f":"F2165*(1-Elteq!$F$6)","v":16.35094331806409}]
["ANAMET-S",8823090,"NPT 1/2\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",50,6.2245068313084877,{"$f":"F2166*(1-Elteq!$F$6)","v":6.2245068313084877}]
["ANAMET-S",8823110,"NPT 1/2\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",50,6.7261835012945452,{"$f":"F2167*(1-Elteq!$F$6)","v":6.7261835012945452}]
["ANAMET-S",8823130,"NPT 1/2\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",50,7.3857954192391757,{"$f":"F2168*(1-Elteq!$F$6)","v":7.3857954192391757}]
["ANAMET-S",8823160,"NPT 1/2\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",50,6.5961191794463083,{"$f":"F2169*(1-Elteq!$F$6)","v":6.5961191794463083}]
["ANAMET-S",8823210,"NPT 3/4\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",50,10.367984513045183,{"$f":"F2170*(1-Elteq!$F$6)","v":10.367984513045183}]
["ANAMET-S",8823260,"NPT 1\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",20,17.43790943636721,{"$f":"F2171*(1-Elteq!$F$6)","v":17.43790943636721}]
["ANAMET-S",8823290,"NPT 1\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",20,18.162553515235963,{"$f":"F2172*(1-Elteq!$F$6)","v":18.162553515235963}]
["ANAMET-S",8823300,"NPT 1 1/4\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",20,18.162553515235963,{"$f":"F2173*(1-Elteq!$F$6)","v":18.162553515235963}]
["ANAMET-S",8823360,"NPT 1 1/4\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",10,18.162553515235963,{"$f":"F2174*(1-Elteq!$F$6)","v":18.162553515235963}]
["ANAMET-S",8823400,"NPT 1 1/2\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",10,22.919191571400059,{"$f":"F2175*(1-Elteq!$F$6)","v":22.919191571400059}]
["ANAMET-S",8823420,"NPT 1 1/2\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",5,55.212304624576632,{"$f":"F2176*(1-Elteq!$F$6)","v":55.212304624576632}]
["ANAMET-S",8823480,"NPT 2\"","Fitting accessories for Sealtite, Adapter NPT/PG nickel plated brass",5,55.212304624576632,{"$f":"F2177*(1-Elteq!$F$6)","v":55.212304624576632}]
["ANAMET-S",8824100,"PG 9","Fitting accessories for Sealtite, Adapter PG/NPT nickel plated brass",50,6.7261835012945452,{"$f":"F2178*(1-Elteq!$F$6)","v":6.7261835012945452}]
["ANAMET-S",8824110,"PG 11","Fitting accessories for Sealtite, Adapter PG/NPT nickel plated brass",50,8.7514707986456646,{"$f":"F2179*(1-Elteq!$F$6)","v":8.7514707986456646}]
["ANAMET-S",8824120,"PG 11","Fitting accessories for Sealtite, Adapter PG/NPT nickel plated brass",50,8.2497941286596088,{"$f":"F2180*(1-Elteq!$F$6)","v":8.2497941286596088}]
["ANAMET-S",8824130,"PG 13,5","Fitting accessories for Sealtite, Adapter PG/NPT nickel plated brass",50,8.1011491894044791,{"$f":"F2181*(1-Elteq!$F$6)","v":8.1011491894044791}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8824160,"PG 16","Fitting accessories for Sealtite, Adapter PG/NPT nickel plated brass",50,8.1011491894044791,{"$f":"F2182*(1-Elteq!$F$6)","v":8.1011491894044791}]
["ANAMET-S",8824200,"PG 21","Fitting accessories for Sealtite, Adapter PG/NPT nickel plated brass",20,13.275851137223626,{"$f":"F2183*(1-Elteq!$F$6)","v":13.275851137223626}]
["ANAMET-S",8824350,"PG 29","Fitting accessories for Sealtite, Adapter PG/NPT nickel plated brass",20,19.621131981676907,{"$f":"F2184*(1-Elteq!$F$6)","v":19.621131981676907}]
["ANAMET-S",8824400,"PG 36","Fitting accessories for Sealtite, Adapter PG/NPT nickel plated brass",10,26.607444126667925,{"$f":"F2185*(1-Elteq!$F$6)","v":26.607444126667925}]
["ANAMET-S",8824500,"PG 48","Fitting accessories for Sealtite, Adapter PG/NPT nickel plated brass",5,73.142600422226451,{"$f":"F2186*(1-Elteq!$F$6)","v":73.142600422226451}]
["ANAMET-S",8825160,"NPT 1/2\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",50,11.659337422824109,{"$f":"F2187*(1-Elteq!$F$6)","v":11.659337422824109}]
["ANAMET-S",8825200,"NPT 1/2\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",50,3.2330274287990353,{"$f":"F2188*(1-Elteq!$F$6)","v":3.2330274287990353}]
["ANAMET-S",8825220,"NPT 1/2\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",50,6.0944425094602499,{"$f":"F2189*(1-Elteq!$F$6)","v":6.0944425094602499}]
["ANAMET-S",8825240,"NPT 3/4\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",50,7.3486341844253937,{"$f":"F2190*(1-Elteq!$F$6)","v":7.3486341844253937}]
["ANAMET-S",8825250,"NPT 3/4\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",50,7.3114729496116118,{"$f":"F2191*(1-Elteq!$F$6)","v":7.3114729496116118}]
["ANAMET-S",8825270,"NPT 3/4\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",10,8.5470840071698628,{"$f":"F2192*(1-Elteq!$F$6)","v":8.5470840071698628}]
["ANAMET-S",8825280,"NPT 1\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",20,12.040240079665375,{"$f":"F2193*(1-Elteq!$F$6)","v":12.040240079665375}]
["ANAMET-S",8825320,"NPT 1\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",20,24.201254172475537,{"$f":"F2194*(1-Elteq!$F$6)","v":24.201254172475537}]
["ANAMET-S",8825360,"NPT 1 1/4\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",20,41.704195769766869,{"$f":"F2195*(1-Elteq!$F$6)","v":41.704195769766869}]
["ANAMET-S",8825380,"NPT 1 1/4\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",10,34.225497263493239,{"$f":"F2196*(1-Elteq!$F$6)","v":34.225497263493239}]
["ANAMET-S",8825400,"NPT 1 1/4\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",20,25.919961282612956,{"$f":"F2197*(1-Elteq!$F$6)","v":25.919961282612956}]
["ANAMET-S",8825480,"NPT 1 1/2\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",1,58.86339594503071,{"$f":"F2198*(1-Elteq!$F$6)","v":58.86339594503071}]
["ANAMET-S",8825500,"NPT 1 1/2\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",1,52.57385695279811,{"$f":"F2199*(1-Elteq!$F$6)","v":52.57385695279811}]
["ANAMET-S",8825520,"NPT 1 1/2\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",1,88.109287743477168,{"$f":"F2200*(1-Elteq!$F$6)","v":88.109287743477168}]
["ANAMET-S",8825600,"NPT 2\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",1,120.96910962756391,{"$f":"F2201*(1-Elteq!$F$6)","v":120.96910962756391}]
["ANAMET-S",8825630,"NPT 2\"","Fitting accessories for Sealtite, Adapter NPT/ISO nickel plated brass",1,91.964765855407038,{"$f":"F2202*(1-Elteq!$F$6)","v":91.964765855407038}]
["ANAMET-S",8826120,"M16 x 1,5","Fitting accessories for Sealtite, Adapter ISO/NPT nickel plated brass",50,5.0910891694881366,{"$f":"F2203*(1-Elteq!$F$6)","v":5.0910891694881366}]
["ANAMET-S",8826160,"M20 x 1,5","Fitting accessories for Sealtite, Adapter ISO/NPT nickel plated brass",50,4.8681217606054448,{"$f":"F2204*(1-Elteq!$F$6)","v":4.8681217606054448}]
["ANAMET-S",8826200,"M25 x 1,5","Fitting accessories for Sealtite, Adapter ISO/NPT nickel plated brass",20,6.2430874487153778,{"$f":"F2205*(1-Elteq!$F$6)","v":6.2430874487153778}]
["ANAMET-S",8826260,"M32 x 1,5","Fitting accessories for Sealtite, Adapter ISO/NPT nickel plated brass",10,7.5623112846046405,{"$f":"F2206*(1-Elteq!$F$6)","v":7.5623112846046405}]
["ANAMET-S",2668120,"3/8\"","Fitting accessories for Sealtite, Encap neoprene",3000,0.45522512646882968,{"$f":"F2207*(1-Elteq!$F$6)","v":0.45522512646882968}]
["ANAMET-S",2668170,"1/2\"","Fitting accessories for Sealtite, Encap neoprene",2400,0.52954759609639368,{"$f":"F2208*(1-Elteq!$F$6)","v":0.52954759609639368}]
["ANAMET-S",2668230,"3/4\"","Fitting accessories for Sealtite, Encap neoprene",1200,0.91045025293765935,{"$f":"F2209*(1-Elteq!$F$6)","v":0.91045025293765935}]
["ANAMET-S",2668290,"1\"","Fitting accessories for Sealtite, Encap neoprene",800,1.2449013662616977,{"$f":"F2210*(1-Elteq!$F$6)","v":1.2449013662616977}]
["ANAMET-S",2668360,"1 1/4\"","Fitting accessories for Sealtite, Encap neoprene",800,1.7651586536546457,{"$f":"F2211*(1-Elteq!$F$6)","v":1.7651586536546457}]
["ANAMET-S",7830160,"M 16 x 1,5","Fitting accessories for Sealtite, Elbow fitting male/female",10,3.0100600199163439,{"$f":"F2212*(1-Elteq!$F$6)","v":3.0100600199163439}]
["ANAMET-S",7830200,"M 20 x 1,5","Fitting accessories for Sealtite, Elbow fitting male/female",10,3.455994837681728,{"$f":"F2213*(1-Elteq!$F$6)","v":3.455994837681728}]
["ANAMET-S",7830250,"M 25 x 1,5","Fitting accessories for Sealtite, Elbow fitting male/female",5,7.1163764668392568,{"$f":"F2214*(1-Elteq!$F$6)","v":7.1163764668392568}]
["ANAMET-S",7830320,"M 32 x 1,5","Fitting accessories for Sealtite, Elbow fitting male/female",5,11.947336992630918,{"$f":"F2215*(1-Elteq!$F$6)","v":11.947336992630918}]
["ANAMET-S",7840100,"-","Fitting accessories for Sealtite, Conduit connector, IP 67",10,6.0851522007568049,{"$f":"F2216*(1-Elteq!$F$6)","v":6.0851522007568049}]
["ANAMET-S",7840120,"-","Fitting accessories for Sealtite, Conduit connector, IP 67",10,5.1561213304122546,{"$f":"F2217*(1-Elteq!$F$6)","v":5.1561213304122546}]
["ANAMET-S",7840160,"-","Fitting accessories for Sealtite, Conduit connector, IP 67",10,6.2709583748257147,{"$f":"F2218*(1-Elteq!$F$6)","v":6.2709583748257147}]
["ANAMET-S",7840200,"-","Fitting accessories for Sealtite, Conduit connector, IP 67",5,9.4296633339971869,{"$f":"F2219*(1-Elteq!$F$6)","v":9.4296633339971869}]
["ANAMET-S",7840260,"-","Fitting accessories for Sealtite, Conduit connector, IP 67",5,16.917652148974263,{"$f":"F2220*(1-Elteq!$F$6)","v":16.917652148974263}]
["ANAMET-S",7840350,"-","Fitting accessories for Sealtite, Conduit connector, IP 67",2,22.696224162517368,{"$f":"F2221*(1-Elteq!$F$6)","v":22.696224162517368}]
["ANAMET-S",7840400,"-","Fitting accessories for Sealtite, Conduit connector, IP 67",2,31.587049591714717,{"$f":"F2222*(1-Elteq!$F$6)","v":31.587049591714717}]
["ANAMET-S",7840500,"-","Fitting accessories for Sealtite, Conduit connector, IP 67",2,44.872191037641784,{"$f":"F2223*(1-Elteq!$F$6)","v":44.872191037641784}]
["ANAMET-S",8852160,"M 16 x 1,5","Fitting accessories for Sealtite, Swivel adapter, IP 54",10,5.5556046046604122,{"$f":"F2224*(1-Elteq!$F$6)","v":5.5556046046604122}]
["ANAMET-S",8852161,"M 16 x 1,5","Fitting accessories for Sealtite, Swivel adapter, IP 67",10,11.44566032264486,{"$f":"F2225*(1-Elteq!$F$6)","v":11.44566032264486}]
["ANAMET-S",8852200,"M 20 x 1,5","Fitting accessories for Sealtite, Swivel adapter, IP 54",10,6.949150910177238,{"$f":"F2226*(1-Elteq!$F$6)","v":6.949150910177238}]
["ANAMET-S",8852201,"M 20 x 1,5","Fitting accessories for Sealtite, Swivel adapter, IP 67",10,14.334946329416413,{"$f":"F2227*(1-Elteq!$F$6)","v":14.334946329416413}]
["ANAMET-S",8852250,"M 25 x 1,5","Fitting accessories for Sealtite, Swivel adapter, IP 54",5,8.3055359808802809,{"$f":"F2228*(1-Elteq!$F$6)","v":8.3055359808802809}]
["ANAMET-S",8852251,"M 25 x 1,5","Fitting accessories for Sealtite, Swivel adapter, IP 67",5,18.719972037442687,{"$f":"F2229*(1-Elteq!$F$6)","v":18.719972037442687}]
["ANAMET-S",8852320,"M 32 x 1,5","Fitting accessories for Sealtite, Swivel adapter, IP 54",5,15.115332260505834,{"$f":"F2230*(1-Elteq!$F$6)","v":15.115332260505834}]
["ANAMET-S",8852321,"M 32 x 1,5","Fitting accessories for Sealtite, Swivel adapter, IP 67",5,24.349899111730668,{"$f":"F2231*(1-Elteq!$F$6)","v":24.349899111730668}]
["ANAMET-S",8852400,"M 40 x 1,5","Fitting accessories for Sealtite, Swivel adapter, IP 54",2,27.443571909978019,{"$f":"F2232*(1-Elteq!$F$6)","v":27.443571909978019}]
["ANAMET-S",8852401,"M 40 x 1,5","Fitting accessories for Sealtite, Swivel adapter, IP 67",2,32.841241266679859,{"$f":"F2233*(1-Elteq!$F$6)","v":32.841241266679859}]
["ANAMET-S",8800119,"PG 11","Fitting accessories for Sealtite, Locknut, stainless steel 304",50,10.079984943238371,{"$f":"F2234*(1-Elteq!$F$6)","v":10.079984943238371}]
["ANAMET-S",8800139,"PG 13,5","Fitting accessories for Sealtite, Locknut, stainless steel 304",10,10.841790256920902,{"$f":"F2235*(1-Elteq!$F$6)","v":10.841790256920902}]
["ANAMET-S",8800169,"PG 16","Fitting accessories for Sealtite, Locknut, stainless steel 304",25,11.222692913762168,{"$f":"F2236*(1-Elteq!$F$6)","v":11.222692913762168}]
["ANAMET-S",8800219,"PG 21","Fitting accessories for Sealtite, Locknut, stainless steel 304",20,19.42603549890455,{"$f":"F2237*(1-Elteq!$F$6)","v":19.42603549890455}]
["ANAMET-S",8800299,"PG 29","Fitting accessories for Sealtite, Locknut, stainless steel 304",5,27.657249010157265,{"$f":"F2238*(1-Elteq!$F$6)","v":27.657249010157265}]
["ANAMET-S",8800369,"PG 36","Fitting accessories for Sealtite, Locknut, stainless steel 304",10,50.037602676757487,{"$f":"F2239*(1-Elteq!$F$6)","v":50.037602676757487}]
["ANAMET-S",8801169,"M16 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 304",50,9.7269532125074427,{"$f":"F2240*(1-Elteq!$F$6)","v":9.7269532125074427}]
["ANAMET-S",8801209,"M20 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 304",50,11.222692913762168,{"$f":"F2241*(1-Elteq!$F$6)","v":11.222692913762168}]
["ANAMET-S",8801259,"M25 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 304",25,13.443076693885644,{"$f":"F2242*(1-Elteq!$F$6)","v":13.443076693885644}]
["ANAMET-S",8801329,"M32 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 304",20,23.903964293965284,{"$f":"F2243*(1-Elteq!$F$6)","v":23.903964293965284}]
["ANAMET-S",8801409,"M40 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 304",5,32.869112192790197,{"$f":"F2244*(1-Elteq!$F$6)","v":32.869112192790197}]
["ANAMET-S",8802169,"NPT 1/2\"","Fitting accessories for Sealtite, Locknut, stainless steel 304",50,11.956627301334363,{"$f":"F2245*(1-Elteq!$F$6)","v":11.956627301334363}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8802209,"NPT 3/4\"","Fitting accessories for Sealtite, Locknut, stainless steel 304",50,14.214172316271622,{"$f":"F2246*(1-Elteq!$F$6)","v":14.214172316271622}]
["ANAMET-S",8802269,"NPT 1 \"","Fitting accessories for Sealtite, Locknut, stainless steel 304",25,25.399703995220008,{"$f":"F2247*(1-Elteq!$F$6)","v":25.399703995220008}]
["ANAMET-S",8802359,"NPT 1 1/4\"","Fitting accessories for Sealtite, Locknut, stainless steel 304",10,34.364851894044918,{"$f":"F2248*(1-Elteq!$F$6)","v":34.364851894044918}]
["ANAMET-S",2972120,"-","Fitting accessories for Sealtite, Ferrule, galvanised steel",50,1.8394811232822097,{"$f":"F2249*(1-Elteq!$F$6)","v":1.8394811232822097}]
["ANAMET-S",2972160,"-","Fitting accessories for Sealtite, Ferrule, galvanised steel",25,1.8394811232822097,{"$f":"F2250*(1-Elteq!$F$6)","v":1.8394811232822097}]
["ANAMET-S",2972200,"-","Fitting accessories for Sealtite, Ferrule, galvanised steel",25,2.0624485321649022,{"$f":"F2251*(1-Elteq!$F$6)","v":2.0624485321649022}]
["ANAMET-S",2972260,"-","Fitting accessories for Sealtite, Ferrule, galvanised steel",25,3.0007697112128979,{"$f":"F2252*(1-Elteq!$F$6)","v":3.0007697112128979}]
["ANAMET-S",2972350,"-","Fitting accessories for Sealtite, Ferrule, galvanised steel",5,7.0234733798048001,{"$f":"F2253*(1-Elteq!$F$6)","v":7.0234733798048001}]
["ANAMET-S",2972400,"-","Fitting accessories for Sealtite, Ferrule, galvanised steel",5,9.0208897510455852,{"$f":"F2254*(1-Elteq!$F$6)","v":9.0208897510455852}]
["ANAMET-S",2972500,"-","Fitting accessories for Sealtite, Ferrule, galvanised steel",5,12.532626440947986,{"$f":"F2255*(1-Elteq!$F$6)","v":12.532626440947986}]
["ANAMET-S",2972630,"-","Fitting accessories for Sealtite, Ferrule, galvanised steel",25,52.945469300935933,{"$f":"F2256*(1-Elteq!$F$6)","v":52.945469300935933}]
["ANAMET-S",2972750,"-","Fitting accessories for Sealtite, Ferrule, galvanised steel",25,71.544667325233831,{"$f":"F2257*(1-Elteq!$F$6)","v":71.544667325233831}]
["ANAMET-S",2972990,"-","Fitting accessories for Sealtite, Ferrule, galvanised steel",1,124.21142736506637,{"$f":"F2258*(1-Elteq!$F$6)","v":124.21142736506637}]
["ANAMET-S",2974160,"-","Fitting accessories for Sealtite, Locknut, galvanised steel",100,0.4273542003584932,{"$f":"F2259*(1-Elteq!$F$6)","v":0.4273542003584932}]
["ANAMET-S",2974200,"-","Fitting accessories for Sealtite, Locknut, galvanised steel",100,0.71535377016530377,{"$f":"F2260*(1-Elteq!$F$6)","v":0.71535377016530377}]
["ANAMET-S",2974260,"-","Fitting accessories for Sealtite, Locknut, galvanised steel",50,1.235611057558252,{"$f":"F2261*(1-Elteq!$F$6)","v":1.235611057558252}]
["ANAMET-S",2974350,"-","Fitting accessories for Sealtite, Locknut, galvanised steel",50,1.4864493925512807,{"$f":"F2262*(1-Elteq!$F$6)","v":1.4864493925512807}]
["ANAMET-S",2974400,"-","Fitting accessories for Sealtite, Locknut, galvanised steel",50,2.2668353236407031,{"$f":"F2263*(1-Elteq!$F$6)","v":2.2668353236407031}]
["ANAMET-S",2974500,"-","Fitting accessories for Sealtite, Locknut, galvanised steel",25,3.4002529854610546,{"$f":"F2264*(1-Elteq!$F$6)","v":3.4002529854610546}]
["ANAMET-S",2974630,"-","Fitting accessories for Sealtite, Locknut, galvanised steel",1,8.8072126508663384,{"$f":"F2265*(1-Elteq!$F$6)","v":8.8072126508663384}]
["ANAMET-S",2974750,"-","Fitting accessories for Sealtite, Locknut, galvanised steel",1,11.25985414857595,{"$f":"F2266*(1-Elteq!$F$6)","v":11.25985414857595}]
["ANAMET-S",2974990,"-","Fitting accessories for Sealtite, Locknut, galvanised steel",1,23.829641824337717,{"$f":"F2267*(1-Elteq!$F$6)","v":23.829641824337717}]
["ANAMET-S",2975120,"-","Fitting accessories for Sealtite, Nut with extrenal lug",25,5.7692817048396581,{"$f":"F2268*(1-Elteq!$F$6)","v":5.7692817048396581}]
["ANAMET-S",2975160,"-","Fitting accessories for Sealtite, Nut with extrenal lug",25,8.8536641943835654,{"$f":"F2269*(1-Elteq!$F$6)","v":8.8536641943835654}]
["ANAMET-S",2975200,"-","Fitting accessories for Sealtite, Nut with extrenal lug",10,15.886427882891812,{"$f":"F2270*(1-Elteq!$F$6)","v":15.886427882891812}]
["ANAMET-S",2975260,"-","Fitting accessories for Sealtite, Nut with extrenal lug",5,24.628608372834034,{"$f":"F2271*(1-Elteq!$F$6)","v":24.628608372834034}]
["ANAMET-S",2975350,"-","Fitting accessories for Sealtite, Nut with extrenal lug",5,62.793196526588162,{"$f":"F2272*(1-Elteq!$F$6)","v":62.793196526588162}]
["ANAMET-S",2975400,"-","Fitting accessories for Sealtite, Nut with extrenal lug",2,63.09048640509841,{"$f":"F2273*(1-Elteq!$F$6)","v":63.09048640509841}]
["ANAMET-S",2975500,"-","Fitting accessories for Sealtite, Nut with extrenal lug",1,70.72712015933061,{"$f":"F2274*(1-Elteq!$F$6)","v":70.72712015933061}]
["ANAMET-S",8150115,"3/8\"","Fitting accessories for Sealtite, Ferrule, stainless steel 304",50,2.6384476717785232,{"$f":"F2275*(1-Elteq!$F$6)","v":2.6384476717785232}]
["ANAMET-S",8150165,"1/2\"","Fitting accessories for Sealtite, Ferrule, stainless steel 304",50,3.1587049591714713,{"$f":"F2276*(1-Elteq!$F$6)","v":3.1587049591714713}]
["ANAMET-S",8150215,"3/4\"","Fitting accessories for Sealtite, Ferrule, stainless steel 304",25,3.6975428639713104,{"$f":"F2277*(1-Elteq!$F$6)","v":3.6975428639713104}]
["ANAMET-S",8150295,"1\"","Fitting accessories for Sealtite, Ferrule, stainless steel 304",25,4.2178001513642585,{"$f":"F2278*(1-Elteq!$F$6)","v":4.2178001513642585}]
["ANAMET-S",8150365,"1 1/4\"","Fitting accessories for Sealtite, Ferrule, stainless steel 304",10,4.5057997211710692,{"$f":"F2279*(1-Elteq!$F$6)","v":4.5057997211710692}]
["ANAMET-S",8150425,"1 1/2\"","Fitting accessories for Sealtite, Ferrule, stainless steel 304",10,4.7194768213503169,{"$f":"F2280*(1-Elteq!$F$6)","v":4.7194768213503169}]
["ANAMET-S",8150485,"2\"","Fitting accessories for Sealtite, Ferrule, stainless steel 304",10,5.917926644094786,{"$f":"F2281*(1-Elteq!$F$6)","v":5.917926644094786}]
["ANAMET-S",8156160,"NPT 1/2\"","Fitting accessories for Sealtite, Seal ring round, NBR",100,5.5741852220673023E-2,{"$f":"F2282*(1-Elteq!$F$6)","v":5.5741852220673023E-2}]
["ANAMET-S",8156200,"NPT 3/4\"","Fitting accessories for Sealtite, Seal ring round, NBR",50,7.4322469627564031E-2,{"$f":"F2283*(1-Elteq!$F$6)","v":7.4322469627564031E-2}]
["ANAMET-S",8156260,"NPT 1\"","Fitting accessories for Sealtite, Seal ring round, NBR",50,8.3612778331009524E-2,{"$f":"F2284*(1-Elteq!$F$6)","v":8.3612778331009524E-2}]
["ANAMET-S",8156350,"NPT 1.1/4\"","Fitting accessories for Sealtite, Seal ring round, NBR",20,0.11148370444134605,{"$f":"F2285*(1-Elteq!$F$6)","v":0.11148370444134605}]
["ANAMET-S",8156400,"NPT 1.1/2\"","Fitting accessories for Sealtite, Seal ring round, NBR",20,0.13006432184823707,{"$f":"F2286*(1-Elteq!$F$6)","v":0.13006432184823707}]
["ANAMET-S",8156500,"NPT 2\"","Fitting accessories for Sealtite, Seal ring round, NBR",20,0.15793524795857358,{"$f":"F2287*(1-Elteq!$F$6)","v":0.15793524795857358}]
["ANAMET-S",8801168,"M16 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 316",50,14.121269229237166,{"$f":"F2288*(1-Elteq!$F$6)","v":14.121269229237166}]
["ANAMET-S",8801208,"M20 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 316",50,16.258040231029632,{"$f":"F2289*(1-Elteq!$F$6)","v":16.258040231029632}]
["ANAMET-S",8801258,"M25 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 316",25,19.46319673371833,{"$f":"F2290*(1-Elteq!$F$6)","v":19.46319673371833}]
["ANAMET-S",8801328,"M32 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 316",20,34.699303007368961,{"$f":"F2291*(1-Elteq!$F$6)","v":34.699303007368961}]
["ANAMET-S",8801408,"M40 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 316",10,47.752186735709884,{"$f":"F2292*(1-Elteq!$F$6)","v":47.752186735709884}]
["ANAMET-S",8802168,"NPT 1/2\"","Fitting accessories for Sealtite, Locknut, stainless steel 316",50,17.326425731925863,{"$f":"F2293*(1-Elteq!$F$6)","v":17.326425731925863}]
["ANAMET-S",8802208,"NPT 3/4\"","Fitting accessories for Sealtite, Locknut, stainless steel 316",50,20.578033778131793,{"$f":"F2294*(1-Elteq!$F$6)","v":20.578033778131793}]
["ANAMET-S",8802268,"NPT 1\"","Fitting accessories for Sealtite, Locknut, stainless steel 316",20,36.836074009161422,{"$f":"F2295*(1-Elteq!$F$6)","v":36.836074009161422}]
["ANAMET-S",8802358,"NPT 1.1/4\"","Fitting accessories for Sealtite, Locknut, stainless steel 316",10,49.888957737502359,{"$f":"F2296*(1-Elteq!$F$6)","v":49.888957737502359}]
["ANAMET-S",8802408,"NPT 1.1/2\"","Fitting accessories for Sealtite, Locknut, stainless steel 316",5,81.290201155148168,{"$f":"F2297*(1-Elteq!$F$6)","v":81.290201155148168}]
["ANAMET-S",8803169,"NPT 1/2\"","Fitting accessories for Sealtite, Locknut, stainless steel 304",100,1.6536749492132996,{"$f":"F2298*(1-Elteq!$F$6)","v":1.6536749492132996}]
["ANAMET-S",8803209,"NPT 3/4\"","Fitting accessories for Sealtite, Locknut, stainless steel 304",50,2.4061899541923855,{"$f":"F2299*(1-Elteq!$F$6)","v":2.4061899541923855}]
["ANAMET-S",8803269,"NPT 1 \"","Fitting accessories for Sealtite, Locknut, stainless steel 304",50,4.2828323122883774,{"$f":"F2300*(1-Elteq!$F$6)","v":4.2828323122883774}]
["ANAMET-S",8803359,"NPT 1 1/4\"","Fitting accessories for Sealtite, Locknut, stainless steel 304",20,4.765928364867543,{"$f":"F2301*(1-Elteq!$F$6)","v":4.765928364867543}]
["ANAMET-S",8803409,"NPT 1 1/2\"","Fitting accessories for Sealtite, Locknut, stainless steel 304",20,6.2245068313084877,{"$f":"F2302*(1-Elteq!$F$6)","v":6.2245068313084877}]
["ANAMET-S",8803509,"NPT 2\"","Fitting accessories for Sealtite, Locknut, stainless steel 304",20,9.6990822863971058,{"$f":"F2303*(1-Elteq!$F$6)","v":9.6990822863971058}]
["ANAMET-S",2970160,"-","Fitting accessories for Sealtite, Sealing gasket, neoprene/steel",100,1.8952229755028829,{"$f":"F2304*(1-Elteq!$F$6)","v":1.8952229755028829}]
["ANAMET-S",2970200,"-","Fitting accessories for Sealtite, Sealing gasket, neoprene/steel",100,1.8952229755028829,{"$f":"F2305*(1-Elteq!$F$6)","v":1.8952229755028829}]
["ANAMET-S",2970260,"-","Fitting accessories for Sealtite, Sealing gasket, neoprene/steel",50,2.9543181676956705,{"$f":"F2306*(1-Elteq!$F$6)","v":2.9543181676956705}]
["ANAMET-S",2970350,"-","Fitting accessories for Sealtite, Sealing gasket, neoprene/steel",50,5.1654116391156997,{"$f":"F2307*(1-Elteq!$F$6)","v":5.1654116391156997}]
["ANAMET-S",2970400,"-","Fitting accessories for Sealtite, Sealing gasket, neoprene/steel",50,6.0758618920533598,{"$f":"F2308*(1-Elteq!$F$6)","v":6.0758618920533598}]
["ANAMET-S",2970500,"-","Fitting accessories for Sealtite, Sealing gasket, neoprene/steel",50,7.4786985062736315,{"$f":"F2309*(1-Elteq!$F$6)","v":7.4786985062736315}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},2973120,"-","Fitting accessories for Sealtite, Wire mesh, galvanised steel",20,44.63993332005564,{"$f":"F2310*(1-Elteq!$F$6)","v":44.63993332005564}]
["ANAMET-S",2973160,"-","Fitting accessories for Sealtite, Wire mesh, galvanised steel",20,47.640703031268544,{"$f":"F2311*(1-Elteq!$F$6)","v":47.640703031268544}]
["ANAMET-S",2973200,"-","Fitting accessories for Sealtite, Wire mesh, galvanised steel",20,57.878623222465485,{"$f":"F2312*(1-Elteq!$F$6)","v":57.878623222465485}]
["ANAMET-S",2973260,"-","Fitting accessories for Sealtite, Wire mesh, galvanised steel",20,64.837064441346186,{"$f":"F2313*(1-Elteq!$F$6)","v":64.837064441346186}]
["ANAMET-S",2973350,"-","Fitting accessories for Sealtite, Wire mesh, galvanised steel",10,74.276018084046797,{"$f":"F2314*(1-Elteq!$F$6)","v":74.276018084046797}]
["ANAMET-S",2973400,"-","Fitting accessories for Sealtite, Wire mesh, galvanised steel",10,108.67803121290551,{"$f":"F2315*(1-Elteq!$F$6)","v":108.67803121290551}]
["ANAMET-S",2973500,"-","Fitting accessories for Sealtite, Wire mesh, galvanised steel",5,163.76956182433736,{"$f":"F2316*(1-Elteq!$F$6)","v":163.76956182433736}]
["ANAMET-S",8850160,"1/2\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",250,0.14864493925512806,{"$f":"F2317*(1-Elteq!$F$6)","v":0.14864493925512806}]
["ANAMET-S",8850162,"1/2\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",100,0.24154802628958311,{"$f":"F2318*(1-Elteq!$F$6)","v":0.24154802628958311}]
["ANAMET-S",8850200,"3/4\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",200,0.2136771001792466,{"$f":"F2319*(1-Elteq!$F$6)","v":0.2136771001792466}]
["ANAMET-S",8850202,"3/4\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",50,0.30658018721370167,{"$f":"F2320*(1-Elteq!$F$6)","v":0.30658018721370167}]
["ANAMET-S",8850260,"1\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",100,0.29728987851025612,{"$f":"F2321*(1-Elteq!$F$6)","v":0.29728987851025612}]
["ANAMET-S",8850262,"1\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",50,0.55741852220673027,{"$f":"F2322*(1-Elteq!$F$6)","v":0.55741852220673027}]
["ANAMET-S",8850350,"1.1/4\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",100,0.35303173073092919,{"$f":"F2323*(1-Elteq!$F$6)","v":0.35303173073092919}]
["ANAMET-S",8850352,"1.1/4\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",50,0.89186963553076837,{"$f":"F2324*(1-Elteq!$F$6)","v":0.89186963553076837}]
["ANAMET-S",8850402,"1.1/2\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",50,0.96619210515833243,{"$f":"F2325*(1-Elteq!$F$6)","v":0.96619210515833243}]
["ANAMET-S",8850502,"2\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",50,1.4492881577374988,{"$f":"F2326*(1-Elteq!$F$6)","v":1.4492881577374988}]
["ANAMET-S",8853060,"1/4\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",100,1.4957397012547262,{"$f":"F2327*(1-Elteq!$F$6)","v":1.4957397012547262}]
["ANAMET-S",8853100,"5/16\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",100,1.5329009360685082,{"$f":"F2328*(1-Elteq!$F$6)","v":1.5329009360685082}]
["ANAMET-S",8853120,"3/8\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",100,1.7930295797649822,{"$f":"F2329*(1-Elteq!$F$6)","v":1.7930295797649822}]
["ANAMET-S",8853160,"1/2\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",100,1.7930295797649822,{"$f":"F2330*(1-Elteq!$F$6)","v":1.7930295797649822}]
["ANAMET-S",8853200,"3/4\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",50,1.9230939016132194,{"$f":"F2331*(1-Elteq!$F$6)","v":1.9230939016132194}]
["ANAMET-S",8853260,"1\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",30,2.2203837801234756,{"$f":"F2332*(1-Elteq!$F$6)","v":2.2203837801234756}]
["ANAMET-S",8853350,"1.1/4\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",20,2.6012864369647408,{"$f":"F2333*(1-Elteq!$F$6)","v":2.6012864369647408}]
["ANAMET-S",8853400,"1.1/2\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",20,3.7997362597092108,{"$f":"F2334*(1-Elteq!$F$6)","v":3.7997362597092108}]
["ANAMET-S",8853500,"2\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",20,5.4998627524397383,{"$f":"F2335*(1-Elteq!$F$6)","v":5.4998627524397383}]
["ANAMET-S",8853630,"2.1/2\"","Fitting accessories for Sealtite, Conduit holder, galvanised steel",1,8.6214064767974268,{"$f":"F2336*(1-Elteq!$F$6)","v":8.6214064767974268}]
["ANAMET-S",3392121,"3/8\"","HFI conduit with blue cover, Stainless steel 304 core with TPU cover",30,17.159200175263845,{"$f":"F2337*(1-Elteq!$F$6)","v":17.159200175263845}]
["ANAMET-S",3392161,"1/2\"","HFI conduit with blue cover, Stainless steel 304 core with TPU cover",30,21.59067742680735,{"$f":"F2338*(1-Elteq!$F$6)","v":21.59067742680735}]
["ANAMET-S",3392201,"3/4\"","HFI conduit with blue cover, Stainless steel 304 core with TPU cover",30,27.517894379605583,{"$f":"F2339*(1-Elteq!$F$6)","v":27.517894379605583}]
["ANAMET-S",3392261,"1\"","HFI conduit with blue cover, Stainless steel 304 core with TPU cover",30,47.863670440151239,{"$f":"F2340*(1-Elteq!$F$6)","v":47.863670440151239}]
["ANAMET-S",3392351,"1 1/4\"","HFI conduit with blue cover, Stainless steel 304 core with TPU cover",15,63.174099183429433,{"$f":"F2341*(1-Elteq!$F$6)","v":63.174099183429433}]
["ANAMET-S",3500121,"3/8\"","AS conduit with black cover, Galvanised steel core with PVC cover",30,7.9432139414459062,{"$f":"F2342*(1-Elteq!$F$6)","v":7.9432139414459062}]
["ANAMET-S",3500161,"1/2\"","AS conduit with black cover, Galvanised steel core with PVC cover",30,9.2438571599282771,{"$f":"F2343*(1-Elteq!$F$6)","v":9.2438571599282771}]
["ANAMET-S",3500201,"3/4\"","AS conduit with black cover, Galvanised steel core with PVC cover",30,13.285141445927071,{"$f":"F2344*(1-Elteq!$F$6)","v":13.285141445927071}]
["ANAMET-S",3500261,"1\"","AS conduit with black cover, Galvanised steel core with PVC cover",30,19.323842103166648,{"$f":"F2345*(1-Elteq!$F$6)","v":19.323842103166648}]
["ANAMET-S",3500351,"1 1/4\"","AS conduit with black cover, Galvanised steel core with PVC cover",15,24.758672694682264,{"$f":"F2346*(1-Elteq!$F$6)","v":24.758672694682264}]
["ANAMET-S",3500401,"1 1/2\"","AS conduit with black cover, Galvanised steel core with PVC cover",15,41.667034534953082,{"$f":"F2347*(1-Elteq!$F$6)","v":41.667034534953082}]
["ANAMET-S",3500501,"2\"","AS conduit with black cover, Galvanised steel core with PVC cover",15,53.605081218880564,{"$f":"F2348*(1-Elteq!$F$6)","v":53.605081218880564}]
["ANAMET-S",8260160,"M 16 x 1,5","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",10,35.795559434375527,{"$f":"F2349*(1-Elteq!$F$6)","v":35.795559434375527}]
["ANAMET-S",8260169,"M 16 x 1,5","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",10,92.810183947420583,{"$f":"F2350*(1-Elteq!$F$6)","v":92.810183947420583}]
["ANAMET-S",8260200,"M 20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",10,36.566655056761498,{"$f":"F2351*(1-Elteq!$F$6)","v":36.566655056761498}]
["ANAMET-S",8260209,"M 20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",10,110.68473789284974,{"$f":"F2352*(1-Elteq!$F$6)","v":110.68473789284974}]
["ANAMET-S",8260250,"M 25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",5,49.331539215295628,{"$f":"F2353*(1-Elteq!$F$6)","v":49.331539215295628}]
["ANAMET-S",8260259,"M 25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",5,131.56935185819523,{"$f":"F2354*(1-Elteq!$F$6)","v":131.56935185819523}]
["ANAMET-S",8260320,"M 32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",5,89.772253001393906,{"$f":"F2355*(1-Elteq!$F$6)","v":89.772253001393906}]
["ANAMET-S",8260329,"M 32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",5,193.03403424019069,{"$f":"F2356*(1-Elteq!$F$6)","v":193.03403424019069}]
["ANAMET-S",8260400,"M 40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",2,114.46589353515205,{"$f":"F2357*(1-Elteq!$F$6)","v":114.46589353515205}]
["ANAMET-S",8260409,"M 40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",2,267.70953559848567,{"$f":"F2358*(1-Elteq!$F$6)","v":267.70953559848567}]
["ANAMET-S",8270120,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",10,35.795559434375527,{"$f":"F2359*(1-Elteq!$F$6)","v":35.795559434375527}]
["ANAMET-S",8270129,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",10,92.810183947420583,{"$f":"F2360*(1-Elteq!$F$6)","v":92.810183947420583}]
["ANAMET-S",8270160,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",10,36.566655056761498,{"$f":"F2361*(1-Elteq!$F$6)","v":36.566655056761498}]
["ANAMET-S",8270169,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",10,110.68473789284974,{"$f":"F2362*(1-Elteq!$F$6)","v":110.68473789284974}]
["ANAMET-S",8270200,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",5,49.331539215295628,{"$f":"F2363*(1-Elteq!$F$6)","v":49.331539215295628}]
["ANAMET-S",8270209,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",5,131.56935185819523,{"$f":"F2364*(1-Elteq!$F$6)","v":131.56935185819523}]
["ANAMET-S",8270260,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",5,89.772253001393906,{"$f":"F2365*(1-Elteq!$F$6)","v":89.772253001393906}]
["ANAMET-S",8270269,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",5,193.03403424019069,{"$f":"F2366*(1-Elteq!$F$6)","v":193.03403424019069}]
["ANAMET-S",8270350,"NPT 1.1/4\"","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",2,114.46589353515205,{"$f":"F2367*(1-Elteq!$F$6)","v":114.46589353515205}]
["ANAMET-S",8270359,"NPT 1.1/4\"","IEC-Ex ATEX fittings for Sealtite, BXA fitting for single wires",2,267.70953559848567,{"$f":"F2368*(1-Elteq!$F$6)","v":267.70953559848567}]
["ANAMET-S",8220080,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",10,26.263702704640441,{"$f":"F2369*(1-Elteq!$F$6)","v":26.263702704640441}]
["ANAMET-S",8220090,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",10,26.263702704640441,{"$f":"F2370*(1-Elteq!$F$6)","v":26.263702704640441}]
["ANAMET-S",8220093,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",10,28.279699693288116,{"$f":"F2371*(1-Elteq!$F$6)","v":28.279699693288116}]
["ANAMET-S",8220100,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",10,24.312737876916884,{"$f":"F2372*(1-Elteq!$F$6)","v":24.312737876916884}]
["ANAMET-S",8220103,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",10,26.198670543716322,{"$f":"F2373*(1-Elteq!$F$6)","v":26.198670543716322}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8220110,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 7-10 mm",10,24.312737876916884,{"$f":"F2374*(1-Elteq!$F$6)","v":24.312737876916884}]
["ANAMET-S",8220113,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 7-10 mm",10,26.198670543716322,{"$f":"F2375*(1-Elteq!$F$6)","v":26.198670543716322}]
["ANAMET-S",8220120,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 5,5-8 mm",10,27.805893949412393,{"$f":"F2376*(1-Elteq!$F$6)","v":27.805893949412393}]
["ANAMET-S",8220123,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 5,5-8 mm",10,29.152988711411989,{"$f":"F2377*(1-Elteq!$F$6)","v":29.152988711411989}]
["ANAMET-S",8220130,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 8-10,5 mm",10,27.805893949412393,{"$f":"F2378*(1-Elteq!$F$6)","v":27.805893949412393}]
["ANAMET-S",8220133,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 8-10,5 mm",10,29.152988711411989,{"$f":"F2379*(1-Elteq!$F$6)","v":29.152988711411989}]
["ANAMET-S",8220140,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",10,27.805893949412393,{"$f":"F2380*(1-Elteq!$F$6)","v":27.805893949412393}]
["ANAMET-S",8220143,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",10,29.152988711411989,{"$f":"F2381*(1-Elteq!$F$6)","v":29.152988711411989}]
["ANAMET-S",8220150,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",5,35.42394708623771,{"$f":"F2382*(1-Elteq!$F$6)","v":35.42394708623771}]
["ANAMET-S",8220153,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",5,37.727943644692189,{"$f":"F2383*(1-Elteq!$F$6)","v":37.727943644692189}]
["ANAMET-S",8220180,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 13-15,5 mm",5,35.42394708623771,{"$f":"F2384*(1-Elteq!$F$6)","v":35.42394708623771}]
["ANAMET-S",8220183,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 13-15,5 mm",5,37.727943644692189,{"$f":"F2385*(1-Elteq!$F$6)","v":37.727943644692189}]
["ANAMET-S",8220190,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15,5-18 mm",5,35.42394708623771,{"$f":"F2386*(1-Elteq!$F$6)","v":35.42394708623771}]
["ANAMET-S",8220193,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15,5-18 mm",5,37.727943644692189,{"$f":"F2387*(1-Elteq!$F$6)","v":37.727943644692189}]
["ANAMET-S",8220230,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15-18 mm",5,72.436536960764585,{"$f":"F2388*(1-Elteq!$F$6)","v":72.436536960764585}]
["ANAMET-S",8220233,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15-18 mm",5,75.76246747659809,{"$f":"F2389*(1-Elteq!$F$6)","v":75.76246747659809}]
["ANAMET-S",8220240,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 18-21 mm",5,72.436536960764585,{"$f":"F2390*(1-Elteq!$F$6)","v":72.436536960764585}]
["ANAMET-S",8220243,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 18-21 mm",5,75.76246747659809,{"$f":"F2391*(1-Elteq!$F$6)","v":75.76246747659809}]
["ANAMET-S",8220250,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-23,5 mm",5,72.436536960764585,{"$f":"F2392*(1-Elteq!$F$6)","v":72.436536960764585}]
["ANAMET-S",8220253,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-23,5 mm",5,75.76246747659809,{"$f":"F2393*(1-Elteq!$F$6)","v":75.76246747659809}]
["ANAMET-S",8220290,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-24 mm",2,105.91880952798221,{"$f":"F2394*(1-Elteq!$F$6)","v":105.91880952798221}]
["ANAMET-S",8220293,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-24 mm",2,113.69479791276608,{"$f":"F2395*(1-Elteq!$F$6)","v":113.69479791276608}]
["ANAMET-S",8220300,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 24-27 mm",2,105.91880952798221,{"$f":"F2396*(1-Elteq!$F$6)","v":105.91880952798221}]
["ANAMET-S",8220303,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 24-27 mm",2,113.69479791276608,{"$f":"F2397*(1-Elteq!$F$6)","v":113.69479791276608}]
["ANAMET-S",8220310,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 27-30 mm",2,105.91880952798221,{"$f":"F2398*(1-Elteq!$F$6)","v":105.91880952798221}]
["ANAMET-S",8220313,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 27-30 mm",2,113.69479791276608,{"$f":"F2399*(1-Elteq!$F$6)","v":113.69479791276608}]
["ANAMET-S",8240100,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",10,24.312737876916884,{"$f":"F2400*(1-Elteq!$F$6)","v":24.312737876916884}]
["ANAMET-S",8240103,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",10,26.198670543716322,{"$f":"F2401*(1-Elteq!$F$6)","v":26.198670543716322}]
["ANAMET-S",8240110,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 7-10 mm",10,24.312737876916884,{"$f":"F2402*(1-Elteq!$F$6)","v":24.312737876916884}]
["ANAMET-S",8240113,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 7-10 mm",10,26.198670543716322,{"$f":"F2403*(1-Elteq!$F$6)","v":26.198670543716322}]
["ANAMET-S",8240120,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 5,5-8 mm",10,27.805893949412393,{"$f":"F2404*(1-Elteq!$F$6)","v":27.805893949412393}]
["ANAMET-S",8240123,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 5,5-8 mm",10,29.152988711411989,{"$f":"F2405*(1-Elteq!$F$6)","v":29.152988711411989}]
["ANAMET-S",8240130,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 8-10,5 mm",10,27.805893949412393,{"$f":"F2406*(1-Elteq!$F$6)","v":27.805893949412393}]
["ANAMET-S",8240133,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 8-10,5 mm",10,29.152988711411989,{"$f":"F2407*(1-Elteq!$F$6)","v":29.152988711411989}]
["ANAMET-S",8240140,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",10,27.805893949412393,{"$f":"F2408*(1-Elteq!$F$6)","v":27.805893949412393}]
["ANAMET-S",8240143,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",10,29.152988711411989,{"$f":"F2409*(1-Elteq!$F$6)","v":29.152988711411989}]
["ANAMET-S",8240150,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",5,35.42394708623771,{"$f":"F2410*(1-Elteq!$F$6)","v":35.42394708623771}]
["ANAMET-S",8240153,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",5,37.727943644692189,{"$f":"F2411*(1-Elteq!$F$6)","v":37.727943644692189}]
["ANAMET-S",8240180,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 13-15,5 mm",5,35.42394708623771,{"$f":"F2412*(1-Elteq!$F$6)","v":35.42394708623771}]
["ANAMET-S",8240183,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 13-15,5 mm",5,37.727943644692189,{"$f":"F2413*(1-Elteq!$F$6)","v":37.727943644692189}]
["ANAMET-S",8240190,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15,5-18 mm",5,35.42394708623771,{"$f":"F2414*(1-Elteq!$F$6)","v":35.42394708623771}]
["ANAMET-S",8240193,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15,5-18 mm",5,37.727943644692189,{"$f":"F2415*(1-Elteq!$F$6)","v":37.727943644692189}]
["ANAMET-S",8240230,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15-18 mm",5,72.436536960764585,{"$f":"F2416*(1-Elteq!$F$6)","v":72.436536960764585}]
["ANAMET-S",8240233,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15-18 mm",5,75.76246747659809,{"$f":"F2417*(1-Elteq!$F$6)","v":75.76246747659809}]
["ANAMET-S",8240240,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 18-21 mm",5,72.436536960764585,{"$f":"F2418*(1-Elteq!$F$6)","v":72.436536960764585}]
["ANAMET-S",8240243,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 18-21 mm",5,75.76246747659809,{"$f":"F2419*(1-Elteq!$F$6)","v":75.76246747659809}]
["ANAMET-S",8240250,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-23,5 mm",5,72.436536960764585,{"$f":"F2420*(1-Elteq!$F$6)","v":72.436536960764585}]
["ANAMET-S",8240253,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-23,5 mm",5,75.76246747659809,{"$f":"F2421*(1-Elteq!$F$6)","v":75.76246747659809}]
["ANAMET-S",8222090,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",10,26.189380235012877,{"$f":"F2422*(1-Elteq!$F$6)","v":26.189380235012877}]
["ANAMET-S",8222093,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",10,28.075312901812314,{"$f":"F2423*(1-Elteq!$F$6)","v":28.075312901812314}]
["ANAMET-S",8222100,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",10,25.167446277633871,{"$f":"F2424*(1-Elteq!$F$6)","v":25.167446277633871}]
["ANAMET-S",8222103,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",10,27.053378944433309,{"$f":"F2425*(1-Elteq!$F$6)","v":27.053378944433309}]
["ANAMET-S",8222110,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 7-10 mm",10,25.167446277633871,{"$f":"F2426*(1-Elteq!$F$6)","v":25.167446277633871}]
["ANAMET-S",8222113,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 7-10 mm",10,27.053378944433309,{"$f":"F2427*(1-Elteq!$F$6)","v":27.053378944433309}]
["ANAMET-S",8222120,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 5,5-8 mm",10,28.837118215494844,{"$f":"F2428*(1-Elteq!$F$6)","v":28.837118215494844}]
["ANAMET-S",8222123,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 5,5-8 mm",10,30.174922668790995,{"$f":"F2429*(1-Elteq!$F$6)","v":30.174922668790995}]
["ANAMET-S",8222130,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 8-10,5 mm",10,28.837118215494844,{"$f":"F2430*(1-Elteq!$F$6)","v":28.837118215494844}]
["ANAMET-S",8222133,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 8-10,5 mm",10,30.174922668790995,{"$f":"F2431*(1-Elteq!$F$6)","v":30.174922668790995}]
["ANAMET-S",8222140,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",10,28.837118215494844,{"$f":"F2432*(1-Elteq!$F$6)","v":28.837118215494844}]
["ANAMET-S",8222143,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",10,30.174922668790995,{"$f":"F2433*(1-Elteq!$F$6)","v":30.174922668790995}]
["ANAMET-S",8222150,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",5,36.761751539533861,{"$f":"F2434*(1-Elteq!$F$6)","v":36.761751539533861}]
["ANAMET-S",8222153,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",5,39.075038406691796,{"$f":"F2435*(1-Elteq!$F$6)","v":39.075038406691796}]
["ANAMET-S",8222180,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 13-15,5 mm",5,36.761751539533861,{"$f":"F2436*(1-Elteq!$F$6)","v":36.761751539533861}]
["ANAMET-S",8222183,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 13-15,5 mm",5,39.075038406691796,{"$f":"F2437*(1-Elteq!$F$6)","v":39.075038406691796}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8222190,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15,5-18 mm",5,36.761751539533861,{"$f":"F2438*(1-Elteq!$F$6)","v":36.761751539533861}]
["ANAMET-S",8222193,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15,5-18 mm",5,39.075038406691796,{"$f":"F2439*(1-Elteq!$F$6)","v":39.075038406691796}]
["ANAMET-S",8222230,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15-18 mm",5,73.783631722764198,{"$f":"F2440*(1-Elteq!$F$6)","v":73.783631722764198}]
["ANAMET-S",8222233,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15-18 mm",5,77.109562238597675,{"$f":"F2441*(1-Elteq!$F$6)","v":77.109562238597675}]
["ANAMET-S",8222240,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 18-21 mm",5,73.783631722764198,{"$f":"F2442*(1-Elteq!$F$6)","v":73.783631722764198}]
["ANAMET-S",8222243,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 18-21 mm",5,77.109562238597675,{"$f":"F2443*(1-Elteq!$F$6)","v":77.109562238597675}]
["ANAMET-S",8222250,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-23,5 mm",5,73.783631722764198,{"$f":"F2444*(1-Elteq!$F$6)","v":73.783631722764198}]
["ANAMET-S",8222253,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-23,5 mm",5,77.109562238597675,{"$f":"F2445*(1-Elteq!$F$6)","v":77.109562238597675}]
["ANAMET-S",8222290,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-24 mm",2,108.43648318661592,{"$f":"F2446*(1-Elteq!$F$6)","v":108.43648318661592}]
["ANAMET-S",8222293,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-24 mm",2,116.2310521888067,{"$f":"F2447*(1-Elteq!$F$6)","v":116.2310521888067}]
["ANAMET-S",8222300,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 24-27 mm",2,108.43648318661592,{"$f":"F2448*(1-Elteq!$F$6)","v":108.43648318661592}]
["ANAMET-S",8222303,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 24-27 mm",2,116.2310521888067,{"$f":"F2449*(1-Elteq!$F$6)","v":116.2310521888067}]
["ANAMET-S",8222310,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 27-30 mm",2,108.43648318661592,{"$f":"F2450*(1-Elteq!$F$6)","v":108.43648318661592}]
["ANAMET-S",8222313,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 27-30 mm",2,116.2310521888067,{"$f":"F2451*(1-Elteq!$F$6)","v":116.2310521888067}]
["ANAMET-S",8242100,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",10,25.167446277633871,{"$f":"F2452*(1-Elteq!$F$6)","v":25.167446277633871}]
["ANAMET-S",8242103,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",10,27.053378944433309,{"$f":"F2453*(1-Elteq!$F$6)","v":27.053378944433309}]
["ANAMET-S",8242110,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 7-10 mm",10,25.167446277633871,{"$f":"F2454*(1-Elteq!$F$6)","v":25.167446277633871}]
["ANAMET-S",8242113,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 7-10 mm",10,27.053378944433309,{"$f":"F2455*(1-Elteq!$F$6)","v":27.053378944433309}]
["ANAMET-S",8242120,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 5,5-8 mm",10,28.837118215494844,{"$f":"F2456*(1-Elteq!$F$6)","v":28.837118215494844}]
["ANAMET-S",8242123,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 5,5-8 mm",10,30.174922668790995,{"$f":"F2457*(1-Elteq!$F$6)","v":30.174922668790995}]
["ANAMET-S",8242130,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 8-10,5 mm",10,28.837118215494844,{"$f":"F2458*(1-Elteq!$F$6)","v":28.837118215494844}]
["ANAMET-S",8242133,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 8-10,5 mm",10,30.174922668790995,{"$f":"F2459*(1-Elteq!$F$6)","v":30.174922668790995}]
["ANAMET-S",8242140,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",10,28.837118215494844,{"$f":"F2460*(1-Elteq!$F$6)","v":28.837118215494844}]
["ANAMET-S",8242143,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",10,30.174922668790995,{"$f":"F2461*(1-Elteq!$F$6)","v":30.174922668790995}]
["ANAMET-S",8242150,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",5,36.761751539533861,{"$f":"F2462*(1-Elteq!$F$6)","v":36.761751539533861}]
["ANAMET-S",8242153,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",5,39.075038406691796,{"$f":"F2463*(1-Elteq!$F$6)","v":39.075038406691796}]
["ANAMET-S",8242180,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 13-15,5 mm",5,36.761751539533861,{"$f":"F2464*(1-Elteq!$F$6)","v":36.761751539533861}]
["ANAMET-S",8242183,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 13-15,5 mm",5,39.075038406691796,{"$f":"F2465*(1-Elteq!$F$6)","v":39.075038406691796}]
["ANAMET-S",8242190,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15,5-18 mm",5,36.761751539533861,{"$f":"F2466*(1-Elteq!$F$6)","v":36.761751539533861}]
["ANAMET-S",8242193,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15,5-18 mm",5,39.075038406691796,{"$f":"F2467*(1-Elteq!$F$6)","v":39.075038406691796}]
["ANAMET-S",8242230,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15-18 mm",5,73.783631722764198,{"$f":"F2468*(1-Elteq!$F$6)","v":73.783631722764198}]
["ANAMET-S",8242233,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15-18 mm",5,77.109562238597675,{"$f":"F2469*(1-Elteq!$F$6)","v":77.109562238597675}]
["ANAMET-S",8242240,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 18-21 mm",5,73.783631722764198,{"$f":"F2470*(1-Elteq!$F$6)","v":73.783631722764198}]
["ANAMET-S",8242243,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 18-21 mm",5,77.109562238597675,{"$f":"F2471*(1-Elteq!$F$6)","v":77.109562238597675}]
["ANAMET-S",8242250,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-23,5 mm",5,73.783631722764198,{"$f":"F2472*(1-Elteq!$F$6)","v":73.783631722764198}]
["ANAMET-S",8242253,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-23,5 mm",5,77.109562238597675,{"$f":"F2473*(1-Elteq!$F$6)","v":77.109562238597675}]
["ANAMET-S",8220096,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",10,98.978948926508409,{"$f":"F2474*(1-Elteq!$F$6)","v":98.978948926508409}]
["ANAMET-S",8220099,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",10,97.148758111929638,{"$f":"F2475*(1-Elteq!$F$6)","v":97.148758111929638}]
["ANAMET-S",8220106,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",10,98.978948926508409,{"$f":"F2476*(1-Elteq!$F$6)","v":98.978948926508409}]
["ANAMET-S",8220109,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",10,97.148758111929638,{"$f":"F2477*(1-Elteq!$F$6)","v":97.148758111929638}]
["ANAMET-S",8220116,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 7-10 mm",10,98.978948926508409,{"$f":"F2478*(1-Elteq!$F$6)","v":98.978948926508409}]
["ANAMET-S",8220119,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 7-10 mm",10,97.148758111929638,{"$f":"F2479*(1-Elteq!$F$6)","v":97.148758111929638}]
["ANAMET-S",8220126,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 5,5-8 mm",10,130.93761086636096,{"$f":"F2480*(1-Elteq!$F$6)","v":130.93761086636096}]
["ANAMET-S",8220129,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 5,5-8 mm",10,129.63696764787855,{"$f":"F2481*(1-Elteq!$F$6)","v":129.63696764787855}]
["ANAMET-S",8220136,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 8-10,5 mm",10,130.93761086636096,{"$f":"F2482*(1-Elteq!$F$6)","v":130.93761086636096}]
["ANAMET-S",8220139,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 8-10,5 mm",10,129.63696764787855,{"$f":"F2483*(1-Elteq!$F$6)","v":129.63696764787855}]
["ANAMET-S",8220146,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",10,130.93761086636096,{"$f":"F2484*(1-Elteq!$F$6)","v":130.93761086636096}]
["ANAMET-S",8220149,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",10,129.63696764787855,{"$f":"F2485*(1-Elteq!$F$6)","v":129.63696764787855}]
["ANAMET-S",8220156,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",5,157.37782943636685,{"$f":"F2486*(1-Elteq!$F$6)","v":157.37782943636685}]
["ANAMET-S",8220159,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",5,155.13886503883649,{"$f":"F2487*(1-Elteq!$F$6)","v":155.13886503883649}]
["ANAMET-S",8220186,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 13-15,5 mm",5,157.37782943636685,{"$f":"F2488*(1-Elteq!$F$6)","v":157.37782943636685}]
["ANAMET-S",8220189,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 13-15,5 mm",5,155.13886503883649,{"$f":"F2489*(1-Elteq!$F$6)","v":155.13886503883649}]
["ANAMET-S",8220196,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15,5-18 mm",5,157.37782943636685,{"$f":"F2490*(1-Elteq!$F$6)","v":157.37782943636685}]
["ANAMET-S",8220199,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15,5-18 mm",5,155.13886503883649,{"$f":"F2491*(1-Elteq!$F$6)","v":155.13886503883649}]
["ANAMET-S",8220236,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15-18 mm",5,234.06003747460602,{"$f":"F2492*(1-Elteq!$F$6)","v":234.06003747460602}]
["ANAMET-S",8220239,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15-18 mm",5,230.82701004580701,{"$f":"F2493*(1-Elteq!$F$6)","v":230.82701004580701}]
["ANAMET-S",8220246,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 18-21 mm",5,234.06003747460602,{"$f":"F2494*(1-Elteq!$F$6)","v":234.06003747460602}]
["ANAMET-S",8220249,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 18-21 mm",5,230.82701004580701,{"$f":"F2495*(1-Elteq!$F$6)","v":230.82701004580701}]
["ANAMET-S",8220256,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-23,5 mm",5,234.06003747460602,{"$f":"F2496*(1-Elteq!$F$6)","v":234.06003747460602}]
["ANAMET-S",8220259,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-23,5 mm",5,230.82701004580701,{"$f":"F2497*(1-Elteq!$F$6)","v":230.82701004580701}]
["ANAMET-S",8220296,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-24 mm",2,358.75456089225156,{"$f":"F2498*(1-Elteq!$F$6)","v":358.75456089225156}]
["ANAMET-S",8220299,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-24 mm",2,351.19224960764689,{"$f":"F2499*(1-Elteq!$F$6)","v":351.19224960764689}]
["ANAMET-S",8220306,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 24-27 mm",2,358.75456089225156,{"$f":"F2500*(1-Elteq!$F$6)","v":358.75456089225156}]
["ANAMET-S",8220309,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 24-27 mm",2,351.19224960764689,{"$f":"F2501*(1-Elteq!$F$6)","v":351.19224960764689}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8220316,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 27-30 mm",2,358.75456089225156,{"$f":"F2502*(1-Elteq!$F$6)","v":358.75456089225156}]
["ANAMET-S",8220319,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 27-30 mm",2,351.19224960764689,{"$f":"F2503*(1-Elteq!$F$6)","v":351.19224960764689}]
["ANAMET-S",8240106,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",10,98.978948926508409,{"$f":"F2504*(1-Elteq!$F$6)","v":98.978948926508409}]
["ANAMET-S",8240109,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 4-7 mm",10,97.148758111929638,{"$f":"F2505*(1-Elteq!$F$6)","v":97.148758111929638}]
["ANAMET-S",8240116,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 7-10 mm",10,98.978948926508409,{"$f":"F2506*(1-Elteq!$F$6)","v":98.978948926508409}]
["ANAMET-S",8240119,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 7-10 mm",10,97.148758111929638,{"$f":"F2507*(1-Elteq!$F$6)","v":97.148758111929638}]
["ANAMET-S",8240126,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 5,5-8 mm",10,130.93761086636096,{"$f":"F2508*(1-Elteq!$F$6)","v":130.93761086636096}]
["ANAMET-S",8240129,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 5,5-8 mm",10,129.63696764787855,{"$f":"F2509*(1-Elteq!$F$6)","v":129.63696764787855}]
["ANAMET-S",8240136,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 8-10,5 mm",10,130.93761086636096,{"$f":"F2510*(1-Elteq!$F$6)","v":130.93761086636096}]
["ANAMET-S",8240139,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 8-10,5 mm",10,129.63696764787855,{"$f":"F2511*(1-Elteq!$F$6)","v":129.63696764787855}]
["ANAMET-S",8240146,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",10,130.93761086636096,{"$f":"F2512*(1-Elteq!$F$6)","v":130.93761086636096}]
["ANAMET-S",8240149,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",10,129.63696764787855,{"$f":"F2513*(1-Elteq!$F$6)","v":129.63696764787855}]
["ANAMET-S",8240156,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",5,157.37782943636685,{"$f":"F2514*(1-Elteq!$F$6)","v":157.37782943636685}]
["ANAMET-S",8240159,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 10,5-13 mm",5,155.13886503883649,{"$f":"F2515*(1-Elteq!$F$6)","v":155.13886503883649}]
["ANAMET-S",8240186,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 13-15,5 mm",5,157.37782943636685,{"$f":"F2516*(1-Elteq!$F$6)","v":157.37782943636685}]
["ANAMET-S",8240189,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 13-15,5 mm",5,155.13886503883649,{"$f":"F2517*(1-Elteq!$F$6)","v":155.13886503883649}]
["ANAMET-S",8240196,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15,5-18 mm",5,157.37782943636685,{"$f":"F2518*(1-Elteq!$F$6)","v":157.37782943636685}]
["ANAMET-S",8240199,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15,5-18 mm",5,155.13886503883649,{"$f":"F2519*(1-Elteq!$F$6)","v":155.13886503883649}]
["ANAMET-S",8240236,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15-18 mm",5,234.06003747460602,{"$f":"F2520*(1-Elteq!$F$6)","v":234.06003747460602}]
["ANAMET-S",8240239,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 15-18 mm",5,230.82701004580701,{"$f":"F2521*(1-Elteq!$F$6)","v":230.82701004580701}]
["ANAMET-S",8240246,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 18-21 mm",5,234.06003747460602,{"$f":"F2522*(1-Elteq!$F$6)","v":234.06003747460602}]
["ANAMET-S",8240249,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 18-21 mm",5,230.82701004580701,{"$f":"F2523*(1-Elteq!$F$6)","v":230.82701004580701}]
["ANAMET-S",8240256,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-23,5 mm",5,234.06003747460602,{"$f":"F2524*(1-Elteq!$F$6)","v":234.06003747460602}]
["ANAMET-S",8240259,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RNA fitting for cable 21-23,5 mm",5,230.82701004580701,{"$f":"F2525*(1-Elteq!$F$6)","v":230.82701004580701}]
["ANAMET-S",8222096,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",10,99.805786401115057,{"$f":"F2526*(1-Elteq!$F$6)","v":99.805786401115057}]
["ANAMET-S",8222099,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",10,97.994176203943184,{"$f":"F2527*(1-Elteq!$F$6)","v":97.994176203943184}]
["ANAMET-S",8222106,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",10,99.805786401115057,{"$f":"F2528*(1-Elteq!$F$6)","v":99.805786401115057}]
["ANAMET-S",8222109,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",10,97.994176203943184,{"$f":"F2529*(1-Elteq!$F$6)","v":97.994176203943184}]
["ANAMET-S",8222116,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 7-10 mm",10,99.805786401115057,{"$f":"F2530*(1-Elteq!$F$6)","v":99.805786401115057}]
["ANAMET-S",8222119,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 7-10 mm",10,97.994176203943184,{"$f":"F2531*(1-Elteq!$F$6)","v":97.994176203943184}]
["ANAMET-S",8222126,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 5,5-8 mm",10,131.92238358892615,{"$f":"F2532*(1-Elteq!$F$6)","v":131.92238358892615}]
["ANAMET-S",8222129,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 5,5-8 mm",10,130.6217403704438,{"$f":"F2533*(1-Elteq!$F$6)","v":130.6217403704438}]
["ANAMET-S",8222136,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 8-10,5 mm",10,131.92238358892615,{"$f":"F2534*(1-Elteq!$F$6)","v":131.92238358892615}]
["ANAMET-S",8222139,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 8-10,5 mm",10,130.6217403704438,{"$f":"F2535*(1-Elteq!$F$6)","v":130.6217403704438}]
["ANAMET-S",8222146,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",10,131.92238358892615,{"$f":"F2536*(1-Elteq!$F$6)","v":131.92238358892615}]
["ANAMET-S",8222149,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",10,130.6217403704438,{"$f":"F2537*(1-Elteq!$F$6)","v":130.6217403704438}]
["ANAMET-S",8222156,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",5,158.67847265484923,{"$f":"F2538*(1-Elteq!$F$6)","v":158.67847265484923}]
["ANAMET-S",8222159,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",5,156.43950825731883,{"$f":"F2539*(1-Elteq!$F$6)","v":156.43950825731883}]
["ANAMET-S",8222186,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 13-15,5 mm",5,158.67847265484923,{"$f":"F2540*(1-Elteq!$F$6)","v":158.67847265484923}]
["ANAMET-S",8222189,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 13-15,5 mm",5,156.43950825731883,{"$f":"F2541*(1-Elteq!$F$6)","v":156.43950825731883}]
["ANAMET-S",8222196,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15,5-18 mm",5,158.67847265484923,{"$f":"F2542*(1-Elteq!$F$6)","v":158.67847265484923}]
["ANAMET-S",8222199,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15,5-18 mm",5,156.43950825731883,{"$f":"F2543*(1-Elteq!$F$6)","v":156.43950825731883}]
["ANAMET-S",8222236,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15-18 mm",5,235.3606806930884,{"$f":"F2544*(1-Elteq!$F$6)","v":235.3606806930884}]
["ANAMET-S",8222239,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15-18 mm",5,232.12765326428936,{"$f":"F2545*(1-Elteq!$F$6)","v":232.12765326428936}]
["ANAMET-S",8222246,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 18-21 mm",5,235.3606806930884,{"$f":"F2546*(1-Elteq!$F$6)","v":235.3606806930884}]
["ANAMET-S",8222249,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 18-21 mm",5,232.12765326428936,{"$f":"F2547*(1-Elteq!$F$6)","v":232.12765326428936}]
["ANAMET-S",8222256,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-23,5 mm",5,235.3606806930884,{"$f":"F2548*(1-Elteq!$F$6)","v":235.3606806930884}]
["ANAMET-S",8222259,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-23,5 mm",5,232.12765326428936,{"$f":"F2549*(1-Elteq!$F$6)","v":232.12765326428936}]
["ANAMET-S",8222296,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-24 mm",2,361.2072023899612,{"$f":"F2550*(1-Elteq!$F$6)","v":361.2072023899612}]
["ANAMET-S",8222299,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-24 mm",2,353.64489110535658,{"$f":"F2551*(1-Elteq!$F$6)","v":353.64489110535658}]
["ANAMET-S",8222306,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 24-27 mm",2,361.2072023899612,{"$f":"F2552*(1-Elteq!$F$6)","v":361.2072023899612}]
["ANAMET-S",8222309,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 24-27 mm",2,353.64489110535658,{"$f":"F2553*(1-Elteq!$F$6)","v":353.64489110535658}]
["ANAMET-S",8222316,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 27-30 mm",2,361.2072023899612,{"$f":"F2554*(1-Elteq!$F$6)","v":361.2072023899612}]
["ANAMET-S",8222319,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 27-30 mm",2,353.64489110535658,{"$f":"F2555*(1-Elteq!$F$6)","v":353.64489110535658}]
["ANAMET-S",8242106,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",10,99.805786401115057,{"$f":"F2556*(1-Elteq!$F$6)","v":99.805786401115057}]
["ANAMET-S",8242109,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 4-7 mm",10,97.994176203943184,{"$f":"F2557*(1-Elteq!$F$6)","v":97.994176203943184}]
["ANAMET-S",8242116,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 7-10 mm",10,99.805786401115057,{"$f":"F2558*(1-Elteq!$F$6)","v":99.805786401115057}]
["ANAMET-S",8242119,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 7-10 mm",10,97.994176203943184,{"$f":"F2559*(1-Elteq!$F$6)","v":97.994176203943184}]
["ANAMET-S",8242126,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 5,5-8 mm",10,131.92238358892615,{"$f":"F2560*(1-Elteq!$F$6)","v":131.92238358892615}]
["ANAMET-S",8242129,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 5,5-8 mm",10,130.6217403704438,{"$f":"F2561*(1-Elteq!$F$6)","v":130.6217403704438}]
["ANAMET-S",8242136,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 8-10,5 mm",10,131.92238358892615,{"$f":"F2562*(1-Elteq!$F$6)","v":131.92238358892615}]
["ANAMET-S",8242139,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 8-10,5 mm",10,130.6217403704438,{"$f":"F2563*(1-Elteq!$F$6)","v":130.6217403704438}]
["ANAMET-S",8242146,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",10,131.92238358892615,{"$f":"F2564*(1-Elteq!$F$6)","v":131.92238358892615}]
["ANAMET-S",8242149,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",10,130.6217403704438,{"$f":"F2565*(1-Elteq!$F$6)","v":130.6217403704438}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8242156,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",5,158.67847265484923,{"$f":"F2566*(1-Elteq!$F$6)","v":158.67847265484923}]
["ANAMET-S",8242159,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 10,5-13 mm",5,156.43950825731883,{"$f":"F2567*(1-Elteq!$F$6)","v":156.43950825731883}]
["ANAMET-S",8242186,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 13-15,5 mm",5,158.67847265484923,{"$f":"F2568*(1-Elteq!$F$6)","v":158.67847265484923}]
["ANAMET-S",8242189,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 13-15,5 mm",5,156.43950825731883,{"$f":"F2569*(1-Elteq!$F$6)","v":156.43950825731883}]
["ANAMET-S",8242196,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15,5-18 mm",5,158.67847265484923,{"$f":"F2570*(1-Elteq!$F$6)","v":158.67847265484923}]
["ANAMET-S",8242199,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15,5-18 mm",5,156.43950825731883,{"$f":"F2571*(1-Elteq!$F$6)","v":156.43950825731883}]
["ANAMET-S",8242236,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15-18 mm",5,235.3606806930884,{"$f":"F2572*(1-Elteq!$F$6)","v":235.3606806930884}]
["ANAMET-S",8242239,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 15-18 mm",5,232.12765326428936,{"$f":"F2573*(1-Elteq!$F$6)","v":232.12765326428936}]
["ANAMET-S",8242246,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 18-21 mm",5,235.3606806930884,{"$f":"F2574*(1-Elteq!$F$6)","v":235.3606806930884}]
["ANAMET-S",8242249,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 18-21 mm",5,232.12765326428936,{"$f":"F2575*(1-Elteq!$F$6)","v":232.12765326428936}]
["ANAMET-S",8242256,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-23,5 mm",5,235.3606806930884,{"$f":"F2576*(1-Elteq!$F$6)","v":235.3606806930884}]
["ANAMET-S",8242259,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, RAA fitting for EMC cable 21-23,5 mm",5,232.12765326428936,{"$f":"F2577*(1-Elteq!$F$6)","v":232.12765326428936}]
["ANAMET-S",8223090,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",10,45.476061103365751,{"$f":"F2578*(1-Elteq!$F$6)","v":45.476061103365751}]
["ANAMET-S",8223093,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",10,46.823155865365344,{"$f":"F2579*(1-Elteq!$F$6)","v":46.823155865365344}]
["ANAMET-S",8223100,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",10,44.454127145986739,{"$f":"F2580*(1-Elteq!$F$6)","v":44.454127145986739}]
["ANAMET-S",8223103,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",10,46.340059812786166,{"$f":"F2581*(1-Elteq!$F$6)","v":46.340059812786166}]
["ANAMET-S",8223110,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 7-10 mm",10,44.454127145986739,{"$f":"F2582*(1-Elteq!$F$6)","v":44.454127145986739}]
["ANAMET-S",8223113,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 7-10 mm",10,46.340059812786166,{"$f":"F2583*(1-Elteq!$F$6)","v":46.340059812786166}]
["ANAMET-S",8223120,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 5,5-8 mm",10,48.225992479585614,{"$f":"F2584*(1-Elteq!$F$6)","v":48.225992479585614}]
["ANAMET-S",8223123,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 5,5-8 mm",10,49.573087241585213,{"$f":"F2585*(1-Elteq!$F$6)","v":49.573087241585213}]
["ANAMET-S",8223130,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 8-10,5 mm",10,48.225992479585614,{"$f":"F2586*(1-Elteq!$F$6)","v":48.225992479585614}]
["ANAMET-S",8223133,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 8-10,5 mm",10,49.573087241585213,{"$f":"F2587*(1-Elteq!$F$6)","v":49.573087241585213}]
["ANAMET-S",8223140,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",10,48.225992479585614,{"$f":"F2588*(1-Elteq!$F$6)","v":48.225992479585614}]
["ANAMET-S",8223143,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",10,49.573087241585213,{"$f":"F2589*(1-Elteq!$F$6)","v":49.573087241585213}]
["ANAMET-S",8223150,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",5,56.420044756024545,{"$f":"F2590*(1-Elteq!$F$6)","v":56.420044756024545}]
["ANAMET-S",8223153,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",5,58.63113822744458,{"$f":"F2591*(1-Elteq!$F$6)","v":58.63113822744458}]
["ANAMET-S",8223180,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 13-15,5 mm",5,56.420044756024545,{"$f":"F2592*(1-Elteq!$F$6)","v":56.420044756024545}]
["ANAMET-S",8223183,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 13-15,5 mm",5,58.63113822744458,{"$f":"F2593*(1-Elteq!$F$6)","v":58.63113822744458}]
["ANAMET-S",8223190,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15,5-18 mm",5,56.420044756024545,{"$f":"F2594*(1-Elteq!$F$6)","v":56.420044756024545}]
["ANAMET-S",8223193,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15,5-18 mm",5,58.63113822744458,{"$f":"F2595*(1-Elteq!$F$6)","v":58.63113822744458}]
["ANAMET-S",8223230,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15-18 mm",5,103.15958784305887,{"$f":"F2596*(1-Elteq!$F$6)","v":103.15958784305887}]
["ANAMET-S",8223233,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15-18 mm",5,106.44835712407858,{"$f":"F2597*(1-Elteq!$F$6)","v":106.44835712407858}]
["ANAMET-S",8223240,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 18-21 mm",5,103.15958784305887,{"$f":"F2598*(1-Elteq!$F$6)","v":103.15958784305887}]
["ANAMET-S",8223243,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 18-21 mm",5,106.44835712407858,{"$f":"F2599*(1-Elteq!$F$6)","v":106.44835712407858}]
["ANAMET-S",8223250,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-23,5 mm",5,103.15958784305887,{"$f":"F2600*(1-Elteq!$F$6)","v":103.15958784305887}]
["ANAMET-S",8223253,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-23,5 mm",5,106.44835712407858,{"$f":"F2601*(1-Elteq!$F$6)","v":106.44835712407858}]
["ANAMET-S",8223290,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-24 mm",2,140.72959623979253,{"$f":"F2602*(1-Elteq!$F$6)","v":140.72959623979253}]
["ANAMET-S",8223293,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-24 mm",2,148.4870040071695,{"$f":"F2603*(1-Elteq!$F$6)","v":148.4870040071695}]
["ANAMET-S",8223300,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 24-27 mm",2,140.72959623979253,{"$f":"F2604*(1-Elteq!$F$6)","v":140.72959623979253}]
["ANAMET-S",8223303,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 24-27 mm",2,148.4870040071695,{"$f":"F2605*(1-Elteq!$F$6)","v":148.4870040071695}]
["ANAMET-S",8223310,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 27-30 mm",2,140.72959623979253,{"$f":"F2606*(1-Elteq!$F$6)","v":140.72959623979253}]
["ANAMET-S",8223313,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 27-30 mm",2,148.4870040071695,{"$f":"F2607*(1-Elteq!$F$6)","v":148.4870040071695}]
["ANAMET-S",8243090,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",10,45.476061103365751,{"$f":"F2608*(1-Elteq!$F$6)","v":45.476061103365751}]
["ANAMET-S",8243093,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",10,46.823155865365344,{"$f":"F2609*(1-Elteq!$F$6)","v":46.823155865365344}]
["ANAMET-S",8243100,"NPT 3/8\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",10,44.454127145986739,{"$f":"F2610*(1-Elteq!$F$6)","v":44.454127145986739}]
["ANAMET-S",8243103,"NPT 3/8\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",10,46.340059812786166,{"$f":"F2611*(1-Elteq!$F$6)","v":46.340059812786166}]
["ANAMET-S",8243110,"NPT 3/8\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 7-10 mm",10,44.454127145986739,{"$f":"F2612*(1-Elteq!$F$6)","v":44.454127145986739}]
["ANAMET-S",8243113,"NPT 3/8\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 7-10 mm",10,46.340059812786166,{"$f":"F2613*(1-Elteq!$F$6)","v":46.340059812786166}]
["ANAMET-S",8243120,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 5,5-8 mm",10,48.225992479585614,{"$f":"F2614*(1-Elteq!$F$6)","v":48.225992479585614}]
["ANAMET-S",8243123,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 5,5-8 mm",10,49.573087241585213,{"$f":"F2615*(1-Elteq!$F$6)","v":49.573087241585213}]
["ANAMET-S",8243130,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 8-10,5 mm",10,48.225992479585614,{"$f":"F2616*(1-Elteq!$F$6)","v":48.225992479585614}]
["ANAMET-S",8243133,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 8-10,5 mm",10,49.573087241585213,{"$f":"F2617*(1-Elteq!$F$6)","v":49.573087241585213}]
["ANAMET-S",8243140,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",10,48.225992479585614,{"$f":"F2618*(1-Elteq!$F$6)","v":48.225992479585614}]
["ANAMET-S",8243143,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",10,49.573087241585213,{"$f":"F2619*(1-Elteq!$F$6)","v":49.573087241585213}]
["ANAMET-S",8243150,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",5,56.420044756024545,{"$f":"F2620*(1-Elteq!$F$6)","v":56.420044756024545}]
["ANAMET-S",8243153,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",5,58.63113822744458,{"$f":"F2621*(1-Elteq!$F$6)","v":58.63113822744458}]
["ANAMET-S",8243180,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 13-15,5 mm",5,56.420044756024545,{"$f":"F2622*(1-Elteq!$F$6)","v":56.420044756024545}]
["ANAMET-S",8243183,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 13-15,5 mm",5,58.63113822744458,{"$f":"F2623*(1-Elteq!$F$6)","v":58.63113822744458}]
["ANAMET-S",8243190,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15,5-18 mm",5,56.420044756024545,{"$f":"F2624*(1-Elteq!$F$6)","v":56.420044756024545}]
["ANAMET-S",8243193,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15,5-18 mm",5,58.63113822744458,{"$f":"F2625*(1-Elteq!$F$6)","v":58.63113822744458}]
["ANAMET-S",8243230,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15-18 mm",5,103.15958784305887,{"$f":"F2626*(1-Elteq!$F$6)","v":103.15958784305887}]
["ANAMET-S",8243233,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15-18 mm",5,106.44835712407858,{"$f":"F2627*(1-Elteq!$F$6)","v":106.44835712407858}]
["ANAMET-S",8243240,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 18-21 mm",5,103.15958784305887,{"$f":"F2628*(1-Elteq!$F$6)","v":103.15958784305887}]
["ANAMET-S",8243243,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 18-21 mm",5,106.44835712407858,{"$f":"F2629*(1-Elteq!$F$6)","v":106.44835712407858}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8243250,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-23,5 mm",5,103.15958784305887,{"$f":"F2630*(1-Elteq!$F$6)","v":103.15958784305887}]
["ANAMET-S",8243253,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-23,5 mm",5,106.44835712407858,{"$f":"F2631*(1-Elteq!$F$6)","v":106.44835712407858}]
["ANAMET-S",8223096,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",10,119.08317696076448,{"$f":"F2632*(1-Elteq!$F$6)","v":119.08317696076448}]
["ANAMET-S",8223099,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",10,117.24369583748226,{"$f":"F2633*(1-Elteq!$F$6)","v":117.24369583748226}]
["ANAMET-S",8223106,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",10,119.08317696076448,{"$f":"F2634*(1-Elteq!$F$6)","v":119.08317696076448}]
["ANAMET-S",8223109,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",10,117.24369583748226,{"$f":"F2635*(1-Elteq!$F$6)","v":117.24369583748226}]
["ANAMET-S",8223116,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 7-10 mm",10,119.08317696076448,{"$f":"F2636*(1-Elteq!$F$6)","v":119.08317696076448}]
["ANAMET-S",8223119,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 7-10 mm",10,117.24369583748226,{"$f":"F2637*(1-Elteq!$F$6)","v":117.24369583748226}]
["ANAMET-S",8223126,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 5,5-8 mm",10,151.29267723561003,{"$f":"F2638*(1-Elteq!$F$6)","v":151.29267723561003}]
["ANAMET-S",8223129,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 5,5-8 mm",10,149.98274370842421,{"$f":"F2639*(1-Elteq!$F$6)","v":149.98274370842421}]
["ANAMET-S",8223136,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 8-10,5 mm",10,151.29267723561003,{"$f":"F2640*(1-Elteq!$F$6)","v":151.29267723561003}]
["ANAMET-S",8223139,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 8-10,5 mm",10,149.98274370842421,{"$f":"F2641*(1-Elteq!$F$6)","v":149.98274370842421}]
["ANAMET-S",8223146,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",10,151.29267723561003,{"$f":"F2642*(1-Elteq!$F$6)","v":151.29267723561003}]
["ANAMET-S",8223149,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",10,149.98274370842421,{"$f":"F2643*(1-Elteq!$F$6)","v":149.98274370842421}]
["ANAMET-S",8223156,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",5,178.04876630153311,{"$f":"F2644*(1-Elteq!$F$6)","v":178.04876630153311}]
["ANAMET-S",8223159,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",5,175.90270499103718,{"$f":"F2645*(1-Elteq!$F$6)","v":175.90270499103718}]
["ANAMET-S",8223186,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 13-15,5 mm",5,178.04876630153311,{"$f":"F2646*(1-Elteq!$F$6)","v":178.04876630153311}]
["ANAMET-S",8223189,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 13-15,5 mm",5,175.90270499103718,{"$f":"F2647*(1-Elteq!$F$6)","v":175.90270499103718}]
["ANAMET-S",8223196,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15,5-18 mm",5,178.04876630153311,{"$f":"F2648*(1-Elteq!$F$6)","v":178.04876630153311}]
["ANAMET-S",8223199,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15,5-18 mm",5,175.90270499103718,{"$f":"F2649*(1-Elteq!$F$6)","v":175.90270499103718}]
["ANAMET-S",8223236,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15-18 mm",5,264.58799187412797,{"$f":"F2650*(1-Elteq!$F$6)","v":264.58799187412797}]
["ANAMET-S",8223239,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15-18 mm",5,261.40141598884617,{"$f":"F2651*(1-Elteq!$F$6)","v":261.40141598884617}]
["ANAMET-S",8223246,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 18-21 mm",5,264.58799187412797,{"$f":"F2652*(1-Elteq!$F$6)","v":264.58799187412797}]
["ANAMET-S",8223249,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 18-21 mm",5,261.40141598884617,{"$f":"F2653*(1-Elteq!$F$6)","v":261.40141598884617}]
["ANAMET-S",8223256,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-23,5 mm",5,264.58799187412797,{"$f":"F2654*(1-Elteq!$F$6)","v":264.58799187412797}]
["ANAMET-S",8223259,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-23,5 mm",5,261.40141598884617,{"$f":"F2655*(1-Elteq!$F$6)","v":261.40141598884617}]
["ANAMET-S",8223296,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-24 mm",2,393.26805772555161,{"$f":"F2656*(1-Elteq!$F$6)","v":393.26805772555161}]
["ANAMET-S",8223299,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-24 mm",2,385.73361736705732,{"$f":"F2657*(1-Elteq!$F$6)","v":385.73361736705732}]
["ANAMET-S",8223306,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 24-27 mm",2,393.26805772555161,{"$f":"F2658*(1-Elteq!$F$6)","v":393.26805772555161}]
["ANAMET-S",8223309,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 24-27 mm",2,385.73361736705732,{"$f":"F2659*(1-Elteq!$F$6)","v":385.73361736705732}]
["ANAMET-S",8223316,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 27-30 mm",2,393.26805772555161,{"$f":"F2660*(1-Elteq!$F$6)","v":393.26805772555161}]
["ANAMET-S",8223319,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 27-30 mm",2,385.73361736705732,{"$f":"F2661*(1-Elteq!$F$6)","v":385.73361736705732}]
["ANAMET-S",8243096,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",10,119.08317696076448,{"$f":"F2662*(1-Elteq!$F$6)","v":119.08317696076448}]
["ANAMET-S",8243099,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",10,117.24369583748226,{"$f":"F2663*(1-Elteq!$F$6)","v":117.24369583748226}]
["ANAMET-S",8243106,"NPT 3/8\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",10,119.08317696076448,{"$f":"F2664*(1-Elteq!$F$6)","v":119.08317696076448}]
["ANAMET-S",8243109,"NPT 3/8\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 4-7 mm",10,117.24369583748226,{"$f":"F2665*(1-Elteq!$F$6)","v":117.24369583748226}]
["ANAMET-S",8243116,"NPT 3/8\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 7-10 mm",10,119.08317696076448,{"$f":"F2666*(1-Elteq!$F$6)","v":119.08317696076448}]
["ANAMET-S",8243119,"NPT 3/8\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 7-10 mm",10,117.24369583748226,{"$f":"F2667*(1-Elteq!$F$6)","v":117.24369583748226}]
["ANAMET-S",8243126,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 5,5-8 mm",10,151.29267723561003,{"$f":"F2668*(1-Elteq!$F$6)","v":151.29267723561003}]
["ANAMET-S",8243129,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 5,5-8 mm",10,149.98274370842421,{"$f":"F2669*(1-Elteq!$F$6)","v":149.98274370842421}]
["ANAMET-S",8243136,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 8-10,5 mm",10,151.29267723561003,{"$f":"F2670*(1-Elteq!$F$6)","v":151.29267723561003}]
["ANAMET-S",8243139,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 8-10,5 mm",10,149.98274370842421,{"$f":"F2671*(1-Elteq!$F$6)","v":149.98274370842421}]
["ANAMET-S",8243146,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",10,151.29267723561003,{"$f":"F2672*(1-Elteq!$F$6)","v":151.29267723561003}]
["ANAMET-S",8243149,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",10,149.98274370842421,{"$f":"F2673*(1-Elteq!$F$6)","v":149.98274370842421}]
["ANAMET-S",8243156,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",5,178.04876630153311,{"$f":"F2674*(1-Elteq!$F$6)","v":178.04876630153311}]
["ANAMET-S",8243159,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 10,5-13 mm",5,175.90270499103718,{"$f":"F2675*(1-Elteq!$F$6)","v":175.90270499103718}]
["ANAMET-S",8243186,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 13-15,5 mm",5,178.04876630153311,{"$f":"F2676*(1-Elteq!$F$6)","v":178.04876630153311}]
["ANAMET-S",8243189,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 13-15,5 mm",5,175.90270499103718,{"$f":"F2677*(1-Elteq!$F$6)","v":175.90270499103718}]
["ANAMET-S",8243196,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15,5-18 mm",5,178.04876630153311,{"$f":"F2678*(1-Elteq!$F$6)","v":178.04876630153311}]
["ANAMET-S",8243199,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15,5-18 mm",5,175.90270499103718,{"$f":"F2679*(1-Elteq!$F$6)","v":175.90270499103718}]
["ANAMET-S",8243236,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15-18 mm",5,264.58799187412797,{"$f":"F2680*(1-Elteq!$F$6)","v":264.58799187412797}]
["ANAMET-S",8243239,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 15-18 mm",5,261.40141598884617,{"$f":"F2681*(1-Elteq!$F$6)","v":261.40141598884617}]
["ANAMET-S",8243246,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 18-21 mm",5,264.58799187412797,{"$f":"F2682*(1-Elteq!$F$6)","v":264.58799187412797}]
["ANAMET-S",8243249,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 18-21 mm",5,261.40141598884617,{"$f":"F2683*(1-Elteq!$F$6)","v":261.40141598884617}]
["ANAMET-S",8243256,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-23,5 mm",5,264.58799187412797,{"$f":"F2684*(1-Elteq!$F$6)","v":264.58799187412797}]
["ANAMET-S",8243259,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, BAA fitting for EMC cable 21-23,5 mm",5,261.40141598884617,{"$f":"F2685*(1-Elteq!$F$6)","v":261.40141598884617}]
["ANAMET-S",8261160,"M 16 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",10,36.427300426209818,{"$f":"F2686*(1-Elteq!$F$6)","v":36.427300426209818}]
["ANAMET-S",8261169,"M 16 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",10,146.87978060147341,{"$f":"F2687*(1-Elteq!$F$6)","v":146.87978060147341}]
["ANAMET-S",8261200,"M 20 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",10,36.427300426209818,{"$f":"F2688*(1-Elteq!$F$6)","v":36.427300426209818}]
["ANAMET-S",8261209,"M 20 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",10,146.87978060147341,{"$f":"F2689*(1-Elteq!$F$6)","v":146.87978060147341}]
["ANAMET-S",8261250,"M 25 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",5,46.358640430193063,{"$f":"F2690*(1-Elteq!$F$6)","v":46.358640430193063}]
["ANAMET-S",8261259,"M 25 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",5,202.97466455287736,{"$f":"F2691*(1-Elteq!$F$6)","v":202.97466455287736}]
["ANAMET-S",8261320,"M 32 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",5,68.646091009758834,{"$f":"F2692*(1-Elteq!$F$6)","v":68.646091009758834}]
["ANAMET-S",8261329,"M 32 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",5,385.05542483170586,{"$f":"F2693*(1-Elteq!$F$6)","v":385.05542483170586}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8261400,"M 40 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",2,117.58743725950973,{"$f":"F2694*(1-Elteq!$F$6)","v":117.58743725950973}]
["ANAMET-S",8261409,"M 40 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",2,413.60454347739386,{"$f":"F2695*(1-Elteq!$F$6)","v":413.60454347739386}]
["ANAMET-S",8261500,"M 50 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",2,143.04288310695043,{"$f":"F2696*(1-Elteq!$F$6)","v":143.04288310695043}]
["ANAMET-S",8261509,"M 50 x 1,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",2,455.94048023899501,{"$f":"F2697*(1-Elteq!$F$6)","v":455.94048023899501}]
["ANAMET-S",8271120,"NPT 1/2\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",10,36.427300426209818,{"$f":"F2698*(1-Elteq!$F$6)","v":36.427300426209818}]
["ANAMET-S",8271129,"NPT 1/2\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",10,146.87978060147341,{"$f":"F2699*(1-Elteq!$F$6)","v":146.87978060147341}]
["ANAMET-S",8271160,"NPT 1/2\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",10,36.427300426209818,{"$f":"F2700*(1-Elteq!$F$6)","v":36.427300426209818}]
["ANAMET-S",8271169,"NPT 1/2\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",10,146.87978060147341,{"$f":"F2701*(1-Elteq!$F$6)","v":146.87978060147341}]
["ANAMET-S",8271200,"NPT 3/4\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",5,46.358640430193063,{"$f":"F2702*(1-Elteq!$F$6)","v":46.358640430193063}]
["ANAMET-S",8271209,"NPT 3/4\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",5,202.97466455287736,{"$f":"F2703*(1-Elteq!$F$6)","v":202.97466455287736}]
["ANAMET-S",8271260,"NPT 1\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",5,68.646091009758834,{"$f":"F2704*(1-Elteq!$F$6)","v":68.646091009758834}]
["ANAMET-S",8271269,"NPT 1\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",5,385.05542483170586,{"$f":"F2705*(1-Elteq!$F$6)","v":385.05542483170586}]
["ANAMET-S",8271350,"NPT 1.1/4\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",2,117.58743725950973,{"$f":"F2706*(1-Elteq!$F$6)","v":117.58743725950973}]
["ANAMET-S",8271359,"NPT 1.1/4\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",2,413.60454347739386,{"$f":"F2707*(1-Elteq!$F$6)","v":413.60454347739386}]
["ANAMET-S",8271400,"NPT 1.1/2\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",2,143.04288310695043,{"$f":"F2708*(1-Elteq!$F$6)","v":143.04288310695043}]
["ANAMET-S",8271409,"NPT 1.1/2\"","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",2,455.94048023899501,{"$f":"F2709*(1-Elteq!$F$6)","v":455.94048023899501}]
["ANAMET-S",8275110,"Pg 11","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",10,36.427300426209818,{"$f":"F2710*(1-Elteq!$F$6)","v":36.427300426209818}]
["ANAMET-S",8275119,"Pg 11","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",10,146.87978060147341,{"$f":"F2711*(1-Elteq!$F$6)","v":146.87978060147341}]
["ANAMET-S",8275130,"Pg 13,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",10,36.427300426209818,{"$f":"F2712*(1-Elteq!$F$6)","v":36.427300426209818}]
["ANAMET-S",8275139,"Pg 13,5","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",10,146.87978060147341,{"$f":"F2713*(1-Elteq!$F$6)","v":146.87978060147341}]
["ANAMET-S",8275160,"Pg 16","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",10,36.427300426209818,{"$f":"F2714*(1-Elteq!$F$6)","v":36.427300426209818}]
["ANAMET-S",8275169,"Pg 16","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",10,146.87978060147341,{"$f":"F2715*(1-Elteq!$F$6)","v":146.87978060147341}]
["ANAMET-S",8275210,"Pg 21","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",5,46.358640430193063,{"$f":"F2716*(1-Elteq!$F$6)","v":46.358640430193063}]
["ANAMET-S",8275219,"Pg 21","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",5,202.97466455287736,{"$f":"F2717*(1-Elteq!$F$6)","v":202.97466455287736}]
["ANAMET-S",8275290,"Pg 29","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",5,68.646091009758834,{"$f":"F2718*(1-Elteq!$F$6)","v":68.646091009758834}]
["ANAMET-S",8275299,"Pg 29","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",5,385.05542483170586,{"$f":"F2719*(1-Elteq!$F$6)","v":385.05542483170586}]
["ANAMET-S",8275360,"Pg 36","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",2,117.58743725950973,{"$f":"F2720*(1-Elteq!$F$6)","v":117.58743725950973}]
["ANAMET-S",8275369,"Pg 36","IEC-Ex ATEX fitting adapters, BXC fitting for single wires",2,413.60454347739386,{"$f":"F2721*(1-Elteq!$F$6)","v":413.60454347739386}]
["ANAMET-S",2978120,"M20 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 5,5-8 mm",10,26.022154678350859,{"$f":"F2722*(1-Elteq!$F$6)","v":26.022154678350859}]
["ANAMET-S",2978130,"M20 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 8-10,5 mm",10,26.022154678350859,{"$f":"F2723*(1-Elteq!$F$6)","v":26.022154678350859}]
["ANAMET-S",2978140,"M20 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 10,5-13 mm",10,26.022154678350859,{"$f":"F2724*(1-Elteq!$F$6)","v":26.022154678350859}]
["ANAMET-S",2978150,"M25 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 10,5-13 mm",5,33.110660219079776,{"$f":"F2725*(1-Elteq!$F$6)","v":33.110660219079776}]
["ANAMET-S",2978180,"M25 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 13-15,5 mm",5,33.110660219079776,{"$f":"F2726*(1-Elteq!$F$6)","v":33.110660219079776}]
["ANAMET-S",2978190,"M25 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 15,5-18 mm",5,33.110660219079776,{"$f":"F2727*(1-Elteq!$F$6)","v":33.110660219079776}]
["ANAMET-S",2978230,"M32 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 15-18 mm",5,49.034249336785372,{"$f":"F2728*(1-Elteq!$F$6)","v":49.034249336785372}]
["ANAMET-S",2978240,"M32 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 18-21 mm",5,49.034249336785372,{"$f":"F2729*(1-Elteq!$F$6)","v":49.034249336785372}]
["ANAMET-S",2978250,"M32 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 21-23,5 mm",5,49.034249336785372,{"$f":"F2730*(1-Elteq!$F$6)","v":49.034249336785372}]
["ANAMET-S",2978290,"M40 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 21-24 mm",2,83.993680987850809,{"$f":"F2731*(1-Elteq!$F$6)","v":83.993680987850809}]
["ANAMET-S",2978300,"M40 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 24-27 mm",2,83.993680987850809,{"$f":"F2732*(1-Elteq!$F$6)","v":83.993680987850809}]
["ANAMET-S",2978310,"M40 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 27-30 mm",2,83.993680987850809,{"$f":"F2733*(1-Elteq!$F$6)","v":83.993680987850809}]
["ANAMET-S",2978430,"M50 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 30-33 mm",1,102.17481512049365,{"$f":"F2734*(1-Elteq!$F$6)","v":102.17481512049365}]
["ANAMET-S",2978440,"M50 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 33-36 mm",1,102.17481512049365,{"$f":"F2735*(1-Elteq!$F$6)","v":102.17481512049365}]
["ANAMET-S",2978510,"M63 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 36-39 mm",1,157.53576468432541,{"$f":"F2736*(1-Elteq!$F$6)","v":157.53576468432541}]
["ANAMET-S",2978520,"M63 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 39-42 mm",1,157.53576468432541,{"$f":"F2737*(1-Elteq!$F$6)","v":157.53576468432541}]
["ANAMET-S",2978530,"M63 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 42-45 mm",1,157.53576468432541,{"$f":"F2738*(1-Elteq!$F$6)","v":157.53576468432541}]
["ANAMET-S",2978540,"M75 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 45-48 mm",1,238.48222441744608,{"$f":"F2739*(1-Elteq!$F$6)","v":238.48222441744608}]
["ANAMET-S",2978550,"M75 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 48-51 mm",1,238.48222441744608,{"$f":"F2740*(1-Elteq!$F$6)","v":238.48222441744608}]
["ANAMET-S",2978560,"M75 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 51-54 mm",1,238.48222441744608,{"$f":"F2741*(1-Elteq!$F$6)","v":238.48222441744608}]
["ANAMET-S",2979120,"NPT 1/2\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 5,5-8 mm",10,26.022154678350859,{"$f":"F2742*(1-Elteq!$F$6)","v":26.022154678350859}]
["ANAMET-S",2979130,"NPT 1/2\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 8-10,5 mm",10,26.022154678350859,{"$f":"F2743*(1-Elteq!$F$6)","v":26.022154678350859}]
["ANAMET-S",2979140,"NPT 1/2\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 10,5-13 mm",10,26.022154678350859,{"$f":"F2744*(1-Elteq!$F$6)","v":26.022154678350859}]
["ANAMET-S",2979150,"NPT 3/4\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 10,5-13 mm",5,33.110660219079776,{"$f":"F2745*(1-Elteq!$F$6)","v":33.110660219079776}]
["ANAMET-S",2979180,"NPT 3/4\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 13-15,5 mm",5,33.110660219079776,{"$f":"F2746*(1-Elteq!$F$6)","v":33.110660219079776}]
["ANAMET-S",2979190,"NPT 3/4\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 15,5-18 mm",5,33.110660219079776,{"$f":"F2747*(1-Elteq!$F$6)","v":33.110660219079776}]
["ANAMET-S",2979230,"NPT 1\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 15-18 mm",5,49.034249336785372,{"$f":"F2748*(1-Elteq!$F$6)","v":49.034249336785372}]
["ANAMET-S",2979240,"NPT 1\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 18-21 mm",5,49.034249336785372,{"$f":"F2749*(1-Elteq!$F$6)","v":49.034249336785372}]
["ANAMET-S",2979250,"NPT 1\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 21-23,5 mm",5,49.034249336785372,{"$f":"F2750*(1-Elteq!$F$6)","v":49.034249336785372}]
["ANAMET-S",2979290,"NPT 1 1/4\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 21-24 mm",2,83.993680987850809,{"$f":"F2751*(1-Elteq!$F$6)","v":83.993680987850809}]
["ANAMET-S",2979300,"NPT 1 1/4\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 24-27 mm",2,83.993680987850809,{"$f":"F2752*(1-Elteq!$F$6)","v":83.993680987850809}]
["ANAMET-S",2979310,"NPT 1 1/4\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 27-30 mm",2,83.993680987850809,{"$f":"F2753*(1-Elteq!$F$6)","v":83.993680987850809}]
["ANAMET-S",2979430,"NPT 1 1/2\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 30-33 mm",1,102.17481512049365,{"$f":"F2754*(1-Elteq!$F$6)","v":102.17481512049365}]
["ANAMET-S",2979440,"NPT 1 1/2\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 33-36 mm",1,102.17481512049365,{"$f":"F2755*(1-Elteq!$F$6)","v":102.17481512049365}]
["ANAMET-S",2979510,"NPT 2\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 36-39 mm",1,157.53576468432541,{"$f":"F2756*(1-Elteq!$F$6)","v":157.53576468432541}]
["ANAMET-S",2979520,"NPT 2\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 39-42 mm",1,157.53576468432541,{"$f":"F2757*(1-Elteq!$F$6)","v":157.53576468432541}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},2979530,"NPT 2\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 42-45 mm",1,157.53576468432541,{"$f":"F2758*(1-Elteq!$F$6)","v":157.53576468432541}]
["ANAMET-S",2979540,"NPT 2.1/2\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 45-48 mm",1,238.48222441744608,{"$f":"F2759*(1-Elteq!$F$6)","v":238.48222441744608}]
["ANAMET-S",2979550,"NPT 2.1/2\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 48-51 mm",1,238.48222441744608,{"$f":"F2760*(1-Elteq!$F$6)","v":238.48222441744608}]
["ANAMET-S",2979560,"NPT 2.1/2\"","IEC-Ex ATEX fitting adapters, RNC fitting for cable 51-54 mm",1,238.48222441744608,{"$f":"F2761*(1-Elteq!$F$6)","v":238.48222441744608}]
["ANAMET-S",2976110,"PG 11","IEC-Ex ATEX fitting adapters, RNC fitting for cable 5,5-8 mm",10,26.022154678350859,{"$f":"F2762*(1-Elteq!$F$6)","v":26.022154678350859}]
["ANAMET-S",2976120,"PG 13,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 5,5-8 mm",10,26.022154678350859,{"$f":"F2763*(1-Elteq!$F$6)","v":26.022154678350859}]
["ANAMET-S",2976130,"PG 13,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 8-10,5 mm",10,26.022154678350859,{"$f":"F2764*(1-Elteq!$F$6)","v":26.022154678350859}]
["ANAMET-S",2976140,"PG 13,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 10,5-13 mm",10,26.022154678350859,{"$f":"F2765*(1-Elteq!$F$6)","v":26.022154678350859}]
["ANAMET-S",2976150,"PG 16","IEC-Ex ATEX fitting adapters, RNC fitting for cable 10,5-13 mm",5,33.110660219079776,{"$f":"F2766*(1-Elteq!$F$6)","v":33.110660219079776}]
["ANAMET-S",2976180,"PG 16","IEC-Ex ATEX fitting adapters, RNC fitting for cable 13-15,5 mm",5,33.110660219079776,{"$f":"F2767*(1-Elteq!$F$6)","v":33.110660219079776}]
["ANAMET-S",2976190,"PG 16","IEC-Ex ATEX fitting adapters, RNC fitting for cable 15,5-18 mm",5,33.110660219079776,{"$f":"F2768*(1-Elteq!$F$6)","v":33.110660219079776}]
["ANAMET-S",2976230,"PG 21","IEC-Ex ATEX fitting adapters, RNC fitting for cable 15-18 mm",5,49.034249336785372,{"$f":"F2769*(1-Elteq!$F$6)","v":49.034249336785372}]
["ANAMET-S",2976240,"PG 21","IEC-Ex ATEX fitting adapters, RNC fitting for cable 18-21 mm",5,49.034249336785372,{"$f":"F2770*(1-Elteq!$F$6)","v":49.034249336785372}]
["ANAMET-S",2976250,"PG 21","IEC-Ex ATEX fitting adapters, RNC fitting for cable 21-23,5 mm",5,49.034249336785372,{"$f":"F2771*(1-Elteq!$F$6)","v":49.034249336785372}]
["ANAMET-S",2976290,"PG 29","IEC-Ex ATEX fitting adapters, RNC fitting for cable 21-24 mm",2,83.993680987850809,{"$f":"F2772*(1-Elteq!$F$6)","v":83.993680987850809}]
["ANAMET-S",2976300,"PG 29","IEC-Ex ATEX fitting adapters, RNC fitting for cable 24-27 mm",2,83.993680987850809,{"$f":"F2773*(1-Elteq!$F$6)","v":83.993680987850809}]
["ANAMET-S",2976310,"PG 29","IEC-Ex ATEX fitting adapters, RNC fitting for cable 27-30 mm",2,83.993680987850809,{"$f":"F2774*(1-Elteq!$F$6)","v":83.993680987850809}]
["ANAMET-S",2976430,"PG 36","IEC-Ex ATEX fitting adapters, RNC fitting for cable 30-33 mm",1,102.17481512049365,{"$f":"F2775*(1-Elteq!$F$6)","v":102.17481512049365}]
["ANAMET-S",2976440,"PG 36","IEC-Ex ATEX fitting adapters, RNC fitting for cable 33-36 mm",1,102.17481512049365,{"$f":"F2776*(1-Elteq!$F$6)","v":102.17481512049365}]
["ANAMET-S",2976510,"PG 48","IEC-Ex ATEX fitting adapters, RNC fitting for cable 36-39 mm",1,157.53576468432541,{"$f":"F2777*(1-Elteq!$F$6)","v":157.53576468432541}]
["ANAMET-S",2976520,"PG 48","IEC-Ex ATEX fitting adapters, RNC fitting for cable 39-42 mm",1,157.53576468432541,{"$f":"F2778*(1-Elteq!$F$6)","v":157.53576468432541}]
["ANAMET-S",2976530,"PG 48","IEC-Ex ATEX fitting adapters, RNC fitting for cable 42-45 mm",1,157.53576468432541,{"$f":"F2779*(1-Elteq!$F$6)","v":157.53576468432541}]
["ANAMET-S",8140401,"NPT 1.1/2\"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",2,26.393767026488675,{"$f":"F2780*(1-Elteq!$F$6)","v":26.393767026488675}]
["ANAMET-S",8140501,"NPT 2\"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",2,41.490518669587622,{"$f":"F2781*(1-Elteq!$F$6)","v":41.490518669587622}]
["ANAMET-S",8144111,"NPT 1/2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,8.4263099940250736,{"$f":"F2782*(1-Elteq!$F$6)","v":8.4263099940250736}]
["ANAMET-S",8144121,"NPT 1/2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,7.2371504799840478,{"$f":"F2783*(1-Elteq!$F$6)","v":7.2371504799840478}]
["ANAMET-S",8144161,"NPT 1/2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,7.7388271499701045,{"$f":"F2784*(1-Elteq!$F$6)","v":7.7388271499701045}]
["ANAMET-S",8144201,"NPT 3/4\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",5,10.470177908783082,{"$f":"F2785*(1-Elteq!$F$6)","v":10.470177908783082}]
["ANAMET-S",8144261,"NPT 1 \"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",5,19.295971177056312,{"$f":"F2786*(1-Elteq!$F$6)","v":19.295971177056312}]
["ANAMET-S",8144351,"NPT 1.1/4 \"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",2,31.271179095797564,{"$f":"F2787*(1-Elteq!$F$6)","v":31.271179095797564}]
["ANAMET-S",8144401,"NPT 1.1/2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",2,40.635810268870635,{"$f":"F2788*(1-Elteq!$F$6)","v":40.635810268870635}]
["ANAMET-S",8144501,"NPT 2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",2,63.397066592312115,{"$f":"F2789*(1-Elteq!$F$6)","v":63.397066592312115}]
["ANAMET-S",8194120,"NPT 1/2\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",10,13.294431754630518,{"$f":"F2790*(1-Elteq!$F$6)","v":13.294431754630518}]
["ANAMET-S",8194160,"NPT 1/2\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",10,17.317135423222421,{"$f":"F2791*(1-Elteq!$F$6)","v":17.317135423222421}]
["ANAMET-S",8194200,"NPT 3/4\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",5,24.730801768571933,{"$f":"F2792*(1-Elteq!$F$6)","v":24.730801768571933}]
["ANAMET-S",8194260,"NPT 1\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",5,39.418779828719273,{"$f":"F2793*(1-Elteq!$F$6)","v":39.418779828719273}]
["ANAMET-S",8199120,"NPT 1/2\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",10,13.294431754630518,{"$f":"F2794*(1-Elteq!$F$6)","v":13.294431754630518}]
["ANAMET-S",8199160,"NPT 1/2\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",10,17.317135423222421,{"$f":"F2795*(1-Elteq!$F$6)","v":17.317135423222421}]
["ANAMET-S",8199200,"NPT 3/4\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",5,24.730801768571933,{"$f":"F2796*(1-Elteq!$F$6)","v":24.730801768571933}]
["ANAMET-S",8199260,"NPT 1\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",5,39.418779828719273,{"$f":"F2797*(1-Elteq!$F$6)","v":39.418779828719273}]
["ANAMET-S",2978129,"M20 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 5,5-8 mm",10,104.91545618801008,{"$f":"F2798*(1-Elteq!$F$6)","v":104.91545618801008}]
["ANAMET-S",2978139,"M20 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 8-10,5 mm",10,104.91545618801008,{"$f":"F2799*(1-Elteq!$F$6)","v":104.91545618801008}]
["ANAMET-S",2978149,"M20 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 10,5-13 mm",10,104.91545618801008,{"$f":"F2800*(1-Elteq!$F$6)","v":104.91545618801008}]
["ANAMET-S",2978159,"M25 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 10,5-13 mm",5,144.98455762597055,{"$f":"F2801*(1-Elteq!$F$6)","v":144.98455762597055}]
["ANAMET-S",2978189,"M25 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 13-15,5 mm",5,144.98455762597055,{"$f":"F2802*(1-Elteq!$F$6)","v":144.98455762597055}]
["ANAMET-S",2978199,"M25 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 15,5-18 mm",5,144.98455762597055,{"$f":"F2803*(1-Elteq!$F$6)","v":144.98455762597055}]
["ANAMET-S",2978239,"M32 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 15-18 mm",5,275.87571694881427,{"$f":"F2804*(1-Elteq!$F$6)","v":275.87571694881427}]
["ANAMET-S",2978249,"M32 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 18-21 mm",5,275.87571694881427,{"$f":"F2805*(1-Elteq!$F$6)","v":275.87571694881427}]
["ANAMET-S",2978259,"M32 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 21-23,5 mm",5,275.87571694881427,{"$f":"F2806*(1-Elteq!$F$6)","v":275.87571694881427}]
["ANAMET-S",2978299,"M40 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 21-24 mm",2,295.43181676956704,{"$f":"F2807*(1-Elteq!$F$6)","v":295.43181676956704}]
["ANAMET-S",2978309,"M40 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 24-27 mm",2,295.43181676956704,{"$f":"F2808*(1-Elteq!$F$6)","v":295.43181676956704}]
["ANAMET-S",2978319,"M40 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 27-30 mm",2,295.43181676956704,{"$f":"F2809*(1-Elteq!$F$6)","v":295.43181676956704}]
["ANAMET-S",2978439,"M50 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 30-33 mm",1,390.80612591913859,{"$f":"F2810*(1-Elteq!$F$6)","v":390.80612591913859}]
["ANAMET-S",2978449,"M50 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 33-36 mm",1,390.80612591913859,{"$f":"F2811*(1-Elteq!$F$6)","v":390.80612591913859}]
["ANAMET-S",2978519,"M63 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 36-39 mm",1,399.88275752240486,{"$f":"F2812*(1-Elteq!$F$6)","v":399.88275752240486}]
["ANAMET-S",2978529,"M63 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 39-42 mm",1,399.88275752240486,{"$f":"F2813*(1-Elteq!$F$6)","v":399.88275752240486}]
["ANAMET-S",2978539,"M63 x 1,5","IEC-Ex ATEX fitting adapters, RNC fitting for cable 42-45 mm",1,399.88275752240486,{"$f":"F2814*(1-Elteq!$F$6)","v":399.88275752240486}]
["ANAMET-S",8140119,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,19.751196303525145,{"$f":"F2815*(1-Elteq!$F$6)","v":19.751196303525145}]
["ANAMET-S",8140129,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,18.562036789484118,{"$f":"F2816*(1-Elteq!$F$6)","v":18.562036789484118}]
["ANAMET-S",8140169,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,26.170799617605986,{"$f":"F2817*(1-Elteq!$F$6)","v":26.170799617605986}]
["ANAMET-S",8140209,"NPT 3/4\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",5,30.091309890459989,{"$f":"F2818*(1-Elteq!$F$6)","v":30.091309890459989}]
["ANAMET-S",8140269,"NPT 1 \"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",5,33.742401210914068,{"$f":"F2819*(1-Elteq!$F$6)","v":33.742401210914068}]
["ANAMET-S",8141129,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",10,25.343962142999338,{"$f":"F2820*(1-Elteq!$F$6)","v":25.343962142999338}]
["ANAMET-S",8141169,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",10,28.892860067715521,{"$f":"F2821*(1-Elteq!$F$6)","v":28.892860067715521}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8141209,"NPT 3/4\"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",5,43.02341960565613,{"$f":"F2822*(1-Elteq!$F$6)","v":43.02341960565613}]
["ANAMET-S",8141269,"NPT 1 \"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",5,57.469849639513889,{"$f":"F2823*(1-Elteq!$F$6)","v":57.469849639513889}]
["ANAMET-S",8192129,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67",10,48.913475323640576,{"$f":"F2824*(1-Elteq!$F$6)","v":48.913475323640576}]
["ANAMET-S",8192169,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67",10,64.196033140808439,{"$f":"F2825*(1-Elteq!$F$6)","v":64.196033140808439}]
["ANAMET-S",8195129,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67",10,48.913475323640576,{"$f":"F2826*(1-Elteq!$F$6)","v":48.913475323640576}]
["ANAMET-S",8195169,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67",10,64.196033140808439,{"$f":"F2827*(1-Elteq!$F$6)","v":64.196033140808439}]
["ANAMET-S",8382209,"NPT 3/4\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67",5,99.034690778729058,{"$f":"F2828*(1-Elteq!$F$6)","v":99.034690778729058}]
["ANAMET-S",8382269,"NPT 1\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67",5,152.10093409280981,{"$f":"F2829*(1-Elteq!$F$6)","v":152.10093409280981}]
["ANAMET-S",8385209,"NPT 3/4\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67",5,99.034690778729058,{"$f":"F2830*(1-Elteq!$F$6)","v":99.034690778729058}]
["ANAMET-S",8385269,"NPT 1\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67",5,152.10093409280981,{"$f":"F2831*(1-Elteq!$F$6)","v":152.10093409280981}]
["ANAMET-S",8140401,"NPT 1.1/2\"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",2,26.393767026488675,{"$f":"F2832*(1-Elteq!$F$6)","v":26.393767026488675}]
["ANAMET-S",8140501,"NPT 2\"","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",2,41.490518669587622,{"$f":"F2833*(1-Elteq!$F$6)","v":41.490518669587622}]
["ANAMET-S",8144111,"NPT 1/2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,8.4263099940250736,{"$f":"F2834*(1-Elteq!$F$6)","v":8.4263099940250736}]
["ANAMET-S",8144121,"NPT 1/2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,7.2371504799840478,{"$f":"F2835*(1-Elteq!$F$6)","v":7.2371504799840478}]
["ANAMET-S",8144161,"NPT 1/2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",10,7.7388271499701045,{"$f":"F2836*(1-Elteq!$F$6)","v":7.7388271499701045}]
["ANAMET-S",8144201,"NPT 3/4\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",5,10.470177908783082,{"$f":"F2837*(1-Elteq!$F$6)","v":10.470177908783082}]
["ANAMET-S",8144261,"NPT 1 \"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",5,19.295971177056312,{"$f":"F2838*(1-Elteq!$F$6)","v":19.295971177056312}]
["ANAMET-S",8144351,"NPT 1.1/4 \"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",2,31.271179095797564,{"$f":"F2839*(1-Elteq!$F$6)","v":31.271179095797564}]
["ANAMET-S",8144401,"NPT 1.1/2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",2,40.635810268870635,{"$f":"F2840*(1-Elteq!$F$6)","v":40.635810268870635}]
["ANAMET-S",8144501,"NPT 2\"","Standard fittings for Sealtite, 45° elbow fixed with male thread, IP 67",2,63.397066592312115,{"$f":"F2841*(1-Elteq!$F$6)","v":63.397066592312115}]
["ANAMET-S",8194120,"NPT 1/2\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",10,13.294431754630518,{"$f":"F2842*(1-Elteq!$F$6)","v":13.294431754630518}]
["ANAMET-S",8194160,"NPT 1/2\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",10,17.317135423222421,{"$f":"F2843*(1-Elteq!$F$6)","v":17.317135423222421}]
["ANAMET-S",8194200,"NPT 3/4\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",5,24.730801768571933,{"$f":"F2844*(1-Elteq!$F$6)","v":24.730801768571933}]
["ANAMET-S",8194260,"NPT 1\"","Swivel fittings for Sealtite, 45° elbow swivel with male thread, IP 67",5,39.418779828719273,{"$f":"F2845*(1-Elteq!$F$6)","v":39.418779828719273}]
["ANAMET-S",8199120,"NPT 1/2\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",10,13.294431754630518,{"$f":"F2846*(1-Elteq!$F$6)","v":13.294431754630518}]
["ANAMET-S",8199160,"NPT 1/2\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",10,17.317135423222421,{"$f":"F2847*(1-Elteq!$F$6)","v":17.317135423222421}]
["ANAMET-S",8199200,"NPT 3/4\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",5,24.730801768571933,{"$f":"F2848*(1-Elteq!$F$6)","v":24.730801768571933}]
["ANAMET-S",8199260,"NPT 1\"","Swivel fittings for Sealtite, 90° elbow swivel with male thread, IP 67",5,39.418779828719273,{"$f":"F2849*(1-Elteq!$F$6)","v":39.418779828719273}]
["ANAMET-S",8218120,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 5,5-8 mm",10,41.239680334594588,{"$f":"F2850*(1-Elteq!$F$6)","v":41.239680334594588}]
["ANAMET-S",8218130,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 8-10,5 mm",10,41.239680334594588,{"$f":"F2851*(1-Elteq!$F$6)","v":41.239680334594588}]
["ANAMET-S",8218140,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 10,5-13 mm",10,41.239680334594588,{"$f":"F2852*(1-Elteq!$F$6)","v":41.239680334594588}]
["ANAMET-S",8218150,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 10,5-13 mm",5,47.649993339971992,{"$f":"F2853*(1-Elteq!$F$6)","v":47.649993339971992}]
["ANAMET-S",8218180,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 13-15,5 mm",5,47.649993339971992,{"$f":"F2854*(1-Elteq!$F$6)","v":47.649993339971992}]
["ANAMET-S",8218190,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 15,5-18 mm",5,47.649993339971992,{"$f":"F2855*(1-Elteq!$F$6)","v":47.649993339971992}]
["ANAMET-S",8218230,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 15-18 mm",5,85.229292045409053,{"$f":"F2856*(1-Elteq!$F$6)","v":85.229292045409053}]
["ANAMET-S",8218240,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 18-21 mm",5,85.229292045409053,{"$f":"F2857*(1-Elteq!$F$6)","v":85.229292045409053}]
["ANAMET-S",8218250,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 21-23,5 mm",5,85.229292045409053,{"$f":"F2858*(1-Elteq!$F$6)","v":85.229292045409053}]
["ANAMET-S",8218290,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 21-24 mm",2,116.66769669786864,{"$f":"F2859*(1-Elteq!$F$6)","v":116.66769669786864}]
["ANAMET-S",8218300,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 24-27 mm",2,116.66769669786864,{"$f":"F2860*(1-Elteq!$F$6)","v":116.66769669786864}]
["ANAMET-S",8218310,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 27-30 mm",2,116.66769669786864,{"$f":"F2861*(1-Elteq!$F$6)","v":116.66769669786864}]
["ANAMET-S",8218430,"M50 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 30-33 mm",1,134.96031453495286,{"$f":"F2862*(1-Elteq!$F$6)","v":134.96031453495286}]
["ANAMET-S",8218440,"M50 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 33-36 mm",1,134.96031453495286,{"$f":"F2863*(1-Elteq!$F$6)","v":134.96031453495286}]
["ANAMET-S",8218510,"M63 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 36-39 mm",1,203.6528570882289,{"$f":"F2864*(1-Elteq!$F$6)","v":203.6528570882289}]
["ANAMET-S",8218520,"M63 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 39-42 mm",1,203.6528570882289,{"$f":"F2865*(1-Elteq!$F$6)","v":203.6528570882289}]
["ANAMET-S",8218530,"M63 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 42-45 mm",1,203.6528570882289,{"$f":"F2866*(1-Elteq!$F$6)","v":203.6528570882289}]
["ANAMET-S",8218540,"M75 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 45-48 mm",1,278.59777739892377,{"$f":"F2867*(1-Elteq!$F$6)","v":278.59777739892377}]
["ANAMET-S",8218550,"M75 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 48-51 mm",1,278.59777739892377,{"$f":"F2868*(1-Elteq!$F$6)","v":278.59777739892377}]
["ANAMET-S",8218560,"M75 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 51-54 mm",1,278.59777739892377,{"$f":"F2869*(1-Elteq!$F$6)","v":278.59777739892377}]
["ANAMET-S",8140119,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,19.751196303525145,{"$f":"F2870*(1-Elteq!$F$6)","v":19.751196303525145}]
["ANAMET-S",8140129,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,18.562036789484118,{"$f":"F2871*(1-Elteq!$F$6)","v":18.562036789484118}]
["ANAMET-S",8140169,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",10,26.170799617605986,{"$f":"F2872*(1-Elteq!$F$6)","v":26.170799617605986}]
["ANAMET-S",8140209,"NPT 3/4\"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",5,30.091309890459989,{"$f":"F2873*(1-Elteq!$F$6)","v":30.091309890459989}]
["ANAMET-S",8140269,"NPT 1 \"","Standard fittings for Sealtite, Stainless steel 304 Straight fixed IP 67",5,33.742401210914068,{"$f":"F2874*(1-Elteq!$F$6)","v":33.742401210914068}]
["ANAMET-S",8141129,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",10,25.343962142999338,{"$f":"F2875*(1-Elteq!$F$6)","v":25.343962142999338}]
["ANAMET-S",8141169,"NPT 1/2\"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",10,28.892860067715521,{"$f":"F2876*(1-Elteq!$F$6)","v":28.892860067715521}]
["ANAMET-S",8141209,"NPT 3/4\"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",5,43.02341960565613,{"$f":"F2877*(1-Elteq!$F$6)","v":43.02341960565613}]
["ANAMET-S",8141269,"NPT 1 \"","Standard fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",5,57.469849639513889,{"$f":"F2878*(1-Elteq!$F$6)","v":57.469849639513889}]
["ANAMET-S",8192129,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67",10,48.913475323640576,{"$f":"F2879*(1-Elteq!$F$6)","v":48.913475323640576}]
["ANAMET-S",8192169,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67",10,64.196033140808439,{"$f":"F2880*(1-Elteq!$F$6)","v":64.196033140808439}]
["ANAMET-S",8195129,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67",10,48.913475323640576,{"$f":"F2881*(1-Elteq!$F$6)","v":48.913475323640576}]
["ANAMET-S",8195169,"NPT 1/2\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67",10,64.196033140808439,{"$f":"F2882*(1-Elteq!$F$6)","v":64.196033140808439}]
["ANAMET-S",8218129,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 5,5-8 mm",10,138.92727635132405,{"$f":"F2883*(1-Elteq!$F$6)","v":138.92727635132405}]
["ANAMET-S",8218139,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 8-10,5 mm",10,138.92727635132405,{"$f":"F2884*(1-Elteq!$F$6)","v":138.92727635132405}]
["ANAMET-S",8218149,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 10,5-13 mm",10,138.92727635132405,{"$f":"F2885*(1-Elteq!$F$6)","v":138.92727635132405}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8218159,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 10,5-13 mm",5,164.42917374228199,{"$f":"F2886*(1-Elteq!$F$6)","v":164.42917374228199}]
["ANAMET-S",8218189,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 13-15,5 mm",5,164.42917374228199,{"$f":"F2887*(1-Elteq!$F$6)","v":164.42917374228199}]
["ANAMET-S",8218199,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 15,5-18 mm",5,164.42917374228199,{"$f":"F2888*(1-Elteq!$F$6)","v":164.42917374228199}]
["ANAMET-S",8218239,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 15-18 mm",5,254.05278180442073,{"$f":"F2889*(1-Elteq!$F$6)","v":254.05278180442073}]
["ANAMET-S",8218249,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 18-21 mm",5,254.05278180442073,{"$f":"F2890*(1-Elteq!$F$6)","v":254.05278180442073}]
["ANAMET-S",8218259,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 21-23,5 mm",5,254.05278180442073,{"$f":"F2891*(1-Elteq!$F$6)","v":254.05278180442073}]
["ANAMET-S",8218299,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 21-24 mm",2,374.41802136626069,{"$f":"F2892*(1-Elteq!$F$6)","v":374.41802136626069}]
["ANAMET-S",8218309,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 24-27 mm",2,374.41802136626069,{"$f":"F2893*(1-Elteq!$F$6)","v":374.41802136626069}]
["ANAMET-S",8218319,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 27-30 mm",2,374.41802136626069,{"$f":"F2894*(1-Elteq!$F$6)","v":374.41802136626069}]
["ANAMET-S",8218439,"M50 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 30-33 mm",1,568.33463493327872,{"$f":"F2895*(1-Elteq!$F$6)","v":568.33463493327872}]
["ANAMET-S",8218449,"M50 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 33-36 mm",1,568.33463493327872,{"$f":"F2896*(1-Elteq!$F$6)","v":568.33463493327872}]
["ANAMET-S",8218519,"M63 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 36-39 mm",1,765.31705037243376,{"$f":"F2897*(1-Elteq!$F$6)","v":765.31705037243376}]
["ANAMET-S",8218529,"M63 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 39-42 mm",1,765.31705037243376,{"$f":"F2898*(1-Elteq!$F$6)","v":765.31705037243376}]
["ANAMET-S",8218539,"M63 x 1,5","IEC-Ex ATEX fittings for Sealtite, BAC fitting for cable 42-45 mm",1,765.31705037243376,{"$f":"F2899*(1-Elteq!$F$6)","v":765.31705037243376}]
["ANAMET-S",8382209,"NPT 3/4\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67",5,99.034690778729058,{"$f":"F2900*(1-Elteq!$F$6)","v":99.034690778729058}]
["ANAMET-S",8382269,"NPT 1\"","Swivel fittings for Sealtite, Stainless 316, 45° elbow swivel, IP 67",5,152.10093409280981,{"$f":"F2901*(1-Elteq!$F$6)","v":152.10093409280981}]
["ANAMET-S",8385209,"NPT 3/4\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67",5,99.034690778729058,{"$f":"F2902*(1-Elteq!$F$6)","v":99.034690778729058}]
["ANAMET-S",8385269,"NPT 1\"","Swivel fittings for Sealtite, Stainless 316, 90° elbow swivel, IP 67",5,152.10093409280981,{"$f":"F2903*(1-Elteq!$F$6)","v":152.10093409280981}]
["ANAMET-S",8262160,"M 16 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",10,33.630917506472727,{"$f":"F2904*(1-Elteq!$F$6)","v":33.630917506472727}]
["ANAMET-S",8262169,"M 16 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",10,107.02435626369221,{"$f":"F2905*(1-Elteq!$F$6)","v":107.02435626369221}]
["ANAMET-S",8262200,"M 20 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",10,35.488979247161829,{"$f":"F2906*(1-Elteq!$F$6)","v":35.488979247161829}]
["ANAMET-S",8262209,"M 20 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",10,130.34303110934044,{"$f":"F2907*(1-Elteq!$F$6)","v":130.34303110934044}]
["ANAMET-S",8262250,"M 25 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",5,41.341873730332495,{"$f":"F2908*(1-Elteq!$F$6)","v":41.341873730332495}]
["ANAMET-S",8262259,"M 25 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",5,156.63460474009119,{"$f":"F2909*(1-Elteq!$F$6)","v":156.63460474009119}]
["ANAMET-S",8262320,"M 32 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",5,78.410205457080053,{"$f":"F2910*(1-Elteq!$F$6)","v":78.410205457080053}]
["ANAMET-S",8262329,"M 32 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",5,219.15838231427944,{"$f":"F2911*(1-Elteq!$F$6)","v":219.15838231427944}]
["ANAMET-S",8262400,"M 40 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",2,100.24243091017699,{"$f":"F2912*(1-Elteq!$F$6)","v":100.24243091017699}]
["ANAMET-S",8262409,"M 40 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",2,282.14667532363995,{"$f":"F2913*(1-Elteq!$F$6)","v":282.14667532363995}]
["ANAMET-S",8262500,"M 50 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",2,111.85531678948388,{"$f":"F2914*(1-Elteq!$F$6)","v":111.85531678948388}]
["ANAMET-S",8262509,"M 50 x 1,5","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",2,353.03173073092916,{"$f":"F2915*(1-Elteq!$F$6)","v":353.03173073092916}]
["ANAMET-S",8272160,"NPT 1/2\"","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",10,35.488979247161829,{"$f":"F2916*(1-Elteq!$F$6)","v":35.488979247161829}]
["ANAMET-S",8272169,"NPT 1/2\"","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",10,130.34303110934044,{"$f":"F2917*(1-Elteq!$F$6)","v":130.34303110934044}]
["ANAMET-S",8272200,"NPT 3/4\"","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",5,41.341873730332495,{"$f":"F2918*(1-Elteq!$F$6)","v":41.341873730332495}]
["ANAMET-S",8272209,"NPT 3/4\"","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",5,156.63460474009119,{"$f":"F2919*(1-Elteq!$F$6)","v":156.63460474009119}]
["ANAMET-S",8272260,"NPT 1\"","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",5,78.410205457080053,{"$f":"F2920*(1-Elteq!$F$6)","v":78.410205457080053}]
["ANAMET-S",8272269,"NPT 1\"","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",5,219.15838231427944,{"$f":"F2921*(1-Elteq!$F$6)","v":219.15838231427944}]
["ANAMET-S",8272350,"NPT 1.1/4\"","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",2,108.60370874327795,{"$f":"F2922*(1-Elteq!$F$6)","v":108.60370874327795}]
["ANAMET-S",8272359,"NPT 1.1/4\"","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",2,290.50795315674088,{"$f":"F2923*(1-Elteq!$F$6)","v":290.50795315674088}]
["ANAMET-S",8272400,"NPT 1.1/2\"","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",2,120.21659462258484,{"$f":"F2924*(1-Elteq!$F$6)","v":120.21659462258484}]
["ANAMET-S",8272409,"NPT 1.1/2\"","IEC-Ex ATEX fitting adapters, BXN fitting for single wires",2,361.39300856403014,{"$f":"F2925*(1-Elteq!$F$6)","v":361.39300856403014}]
["ANAMET-S",7812200,"M 16 X 1,5","IEC-Ex ATEX fittings for Sealtite, Enlarger ISO/ISO nickel plated brass",10,25.055962573192524,{"$f":"F2926*(1-Elteq!$F$6)","v":25.055962573192524}]
["ANAMET-S",7812250,"M 20 X 1,5","IEC-Ex ATEX fittings for Sealtite, Enlarger ISO/ISO nickel plated brass",10,24.57286652061336,{"$f":"F2927*(1-Elteq!$F$6)","v":24.57286652061336}]
["ANAMET-S",7812320,"M 25 X 1,5","IEC-Ex ATEX fittings for Sealtite, Enlarger ISO/ISO nickel plated brass",5,29.589633220473932,{"$f":"F2928*(1-Elteq!$F$6)","v":29.589633220473932}]
["ANAMET-S",7812400,"M 32 X 1,5","IEC-Ex ATEX fittings for Sealtite, Enlarger ISO/ISO nickel plated brass",2,38.694135749850524,{"$f":"F2929*(1-Elteq!$F$6)","v":38.694135749850524}]
["ANAMET-S",7812500,"M 40 X 1,5","IEC-Ex ATEX fittings for Sealtite, Enlarger ISO/ISO nickel plated brass",2,59.708814037044249,{"$f":"F2930*(1-Elteq!$F$6)","v":59.708814037044249}]
["ANAMET-S",7812630,"M 50 X 1,5","IEC-Ex ATEX fittings for Sealtite, Enlarger ISO/ISO nickel plated brass",2,90.115994423421384,{"$f":"F2931*(1-Elteq!$F$6)","v":90.115994423421384}]
["ANAMET-S",7822160,"M 20 X 1,5","IEC-Ex ATEX fittings for Sealtite, Reducer ISO/ISO nickel plated brass",10,25.055962573192524,{"$f":"F2932*(1-Elteq!$F$6)","v":25.055962573192524}]
["ANAMET-S",7822200,"M 25 X 1,5","IEC-Ex ATEX fittings for Sealtite, Reducer ISO/ISO nickel plated brass",10,22.789127249551822,{"$f":"F2933*(1-Elteq!$F$6)","v":22.789127249551822}]
["ANAMET-S",7822250,"M 32 X 1,5","IEC-Ex ATEX fittings for Sealtite, Reducer ISO/ISO nickel plated brass",5,27.694410244971049,{"$f":"F2934*(1-Elteq!$F$6)","v":27.694410244971049}]
["ANAMET-S",7822320,"M 40 X 1,5","IEC-Ex ATEX fittings for Sealtite, Reducer ISO/ISO nickel plated brass",5,35.033754120692997,{"$f":"F2935*(1-Elteq!$F$6)","v":35.033754120692997}]
["ANAMET-S",7822400,"M 50 X 1,5","IEC-Ex ATEX fittings for Sealtite, Reducer ISO/ISO nickel plated brass",1,48.225992479585614,{"$f":"F2936*(1-Elteq!$F$6)","v":48.225992479585614}]
["ANAMET-S",7822500,"M 63 X 1,5","IEC-Ex ATEX fittings for Sealtite, Reducer ISO/ISO nickel plated brass",1,80.630589237203523,{"$f":"F2937*(1-Elteq!$F$6)","v":80.630589237203523}]
["ANAMET-S",8801160,"M16 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",50,0.20438679147580111,{"$f":"F2938*(1-Elteq!$F$6)","v":0.20438679147580111}]
["ANAMET-S",8801200,"M20 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",50,0.27870926110336514,{"$f":"F2939*(1-Elteq!$F$6)","v":0.27870926110336514}]
["ANAMET-S",8801250,"M25 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",25,0.39948327424815672,{"$f":"F2940*(1-Elteq!$F$6)","v":0.39948327424815672}]
["ANAMET-S",8801320,"M32 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",20,0.5016766699860572,{"$f":"F2941*(1-Elteq!$F$6)","v":0.5016766699860572}]
["ANAMET-S",8801400,"M40 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",10,1.2449013662616977,{"$f":"F2942*(1-Elteq!$F$6)","v":1.2449013662616977}]
["ANAMET-S",8801500,"M50 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",10,2.0067066799442288,{"$f":"F2943*(1-Elteq!$F$6)","v":2.0067066799442288}]
["ANAMET-S",8801630,"M63 x 1,5","Fitting accessories for Sealtite, Locknut, nickel plated brass",5,2.8242538458474336,{"$f":"F2944*(1-Elteq!$F$6)","v":2.8242538458474336}]
["ANAMET-S",8802160,"NPT 1/2\"","Fitting accessories for Sealtite, Locknut, nickel plated brass",50,0.5202572873929483,{"$f":"F2945*(1-Elteq!$F$6)","v":0.5202572873929483}]
["ANAMET-S",8802200,"NPT 3/4\"","Fitting accessories for Sealtite, Locknut, nickel plated brass",20,0.65961191794463081,{"$f":"F2946*(1-Elteq!$F$6)","v":0.65961191794463081}]
["ANAMET-S",8802260,"NPT 1 \"","Fitting accessories for Sealtite, Locknut, nickel plated brass",20,1.124127353116906,{"$f":"F2947*(1-Elteq!$F$6)","v":1.124127353116906}]
["ANAMET-S",8802350,"NPT 1 1/4\"","Fitting accessories for Sealtite, Locknut, nickel plated brass",25,1.6350943318064088,{"$f":"F2948*(1-Elteq!$F$6)","v":1.6350943318064088}]
["ANAMET-S",8802400,"NPT 1 1/2\"","Fitting accessories for Sealtite, Locknut, nickel plated brass",10,2.8799956980681065,{"$f":"F2949*(1-Elteq!$F$6)","v":2.8799956980681065}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8802500,"NPT 2\"","Fitting accessories for Sealtite, Locknut, nickel plated brass",10,5.6020561481776392,{"$f":"F2950*(1-Elteq!$F$6)","v":5.6020561481776392}]
["ANAMET-S",8805100,"M16 x 1,5 / NPT 3/8\"","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",50,5.3883790479983924,{"$f":"F2951*(1-Elteq!$F$6)","v":5.3883790479983924}]
["ANAMET-S",8805110,"PG 11","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",50,5.3883790479983924,{"$f":"F2952*(1-Elteq!$F$6)","v":5.3883790479983924}]
["ANAMET-S",8805120,"M20  / PG13,5 / NPT1/2\"","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",50,5.3883790479983924,{"$f":"F2953*(1-Elteq!$F$6)","v":5.3883790479983924}]
["ANAMET-S",8805130,"M25 x 1,5  / NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",50,5.7135398526189851,{"$f":"F2954*(1-Elteq!$F$6)","v":5.7135398526189851}]
["ANAMET-S",8805160,"PG 16","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",50,5.7135398526189851,{"$f":"F2955*(1-Elteq!$F$6)","v":5.7135398526189851}]
["ANAMET-S",8805200,"M32 x 1,5 / NPT 1\"","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",50,7.5994725194184216,{"$f":"F2956*(1-Elteq!$F$6)","v":7.5994725194184216}]
["ANAMET-S",8805210,"PG 21","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",50,7.5994725194184216,{"$f":"F2957*(1-Elteq!$F$6)","v":7.5994725194184216}]
["ANAMET-S",8805250,"NPT 1.1/4”","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",50,10.182178338976273,{"$f":"F2958*(1-Elteq!$F$6)","v":10.182178338976273}]
["ANAMET-S",8805270,"M40 x 1,5","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",50,10.182178338976273,{"$f":"F2959*(1-Elteq!$F$6)","v":10.182178338976273}]
["ANAMET-S",8805290,"Pg 29","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",50,10.182178338976273,{"$f":"F2960*(1-Elteq!$F$6)","v":10.182178338976273}]
["ANAMET-S",8805320,"NPT 1.1/2”","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",50,12.616239219278995,{"$f":"F2961*(1-Elteq!$F$6)","v":12.616239219278995}]
["ANAMET-S",8805350,"M50 x 1,5","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",50,12.616239219278995,{"$f":"F2962*(1-Elteq!$F$6)","v":12.616239219278995}]
["ANAMET-S",8805360,"Pg 36","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",50,12.616239219278995,{"$f":"F2963*(1-Elteq!$F$6)","v":12.616239219278995}]
["ANAMET-S",8805420,"Pg 42","IEC-Ex ATEX fittings for Sealtite, Earthning tags, nickel plated brass",50,12.616239219278995,{"$f":"F2964*(1-Elteq!$F$6)","v":12.616239219278995}]
["ANAMET-S",7811110,"M 20 X 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/PG nickel plated brass",10,25.055962573192524,{"$f":"F2965*(1-Elteq!$F$6)","v":25.055962573192524}]
["ANAMET-S",7811150,"M 20 X 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/PG nickel plated brass",10,24.57286652061336,{"$f":"F2966*(1-Elteq!$F$6)","v":24.57286652061336}]
["ANAMET-S",7811160,"M 25 X 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/PG nickel plated brass",10,24.57286652061336,{"$f":"F2967*(1-Elteq!$F$6)","v":24.57286652061336}]
["ANAMET-S",7811180,"M 25 X 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/PG nickel plated brass",5,27.694410244971049,{"$f":"F2968*(1-Elteq!$F$6)","v":27.694410244971049}]
["ANAMET-S",7811210,"M 32 X 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/PG nickel plated brass",5,29.589633220473932,{"$f":"F2969*(1-Elteq!$F$6)","v":29.589633220473932}]
["ANAMET-S",7811290,"M 40 X 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/PG nickel plated brass",2,38.694135749850524,{"$f":"F2970*(1-Elteq!$F$6)","v":38.694135749850524}]
["ANAMET-S",7811360,"M50 x 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/PG nickel plated brass",1,59.708814037044249,{"$f":"F2971*(1-Elteq!$F$6)","v":59.708814037044249}]
["ANAMET-S",7811480,"M63 x 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/PG nickel plated brass",1,127.67671251145158,{"$f":"F2972*(1-Elteq!$F$6)","v":127.67671251145158}]
["ANAMET-S",7821110,"PG 11","IEC-Ex ATEX fittings for Sealtite, Adapter PG/ISO nickel plated brass",10,25.055962573192524,{"$f":"F2973*(1-Elteq!$F$6)","v":25.055962573192524}]
["ANAMET-S",7821160,"PG 16","IEC-Ex ATEX fittings for Sealtite, Adapter PG/ISO nickel plated brass",10,24.57286652061336,{"$f":"F2974*(1-Elteq!$F$6)","v":24.57286652061336}]
["ANAMET-S",7821210,"PG 21","IEC-Ex ATEX fittings for Sealtite, Adapter PG/ISO nickel plated brass",5,27.694410244971049,{"$f":"F2975*(1-Elteq!$F$6)","v":27.694410244971049}]
["ANAMET-S",7821290,"PG 29","IEC-Ex ATEX fittings for Sealtite, Adapter PG/ISO nickel plated brass",5,35.033754120692997,{"$f":"F2976*(1-Elteq!$F$6)","v":35.033754120692997}]
["ANAMET-S",7821360,"PG 36","IEC-Ex ATEX fittings for Sealtite, Adapter PG/ISO nickel plated brass",1,48.225992479585614,{"$f":"F2977*(1-Elteq!$F$6)","v":48.225992479585614}]
["ANAMET-S",7824110,"PG 11","IEC-Ex ATEX fittings for Sealtite, Adapter PG/NPT nickel plated brass",10,25.055962573192524,{"$f":"F2978*(1-Elteq!$F$6)","v":25.055962573192524}]
["ANAMET-S",7824120,"PG 11","IEC-Ex ATEX fittings for Sealtite, Adapter PG/NPT nickel plated brass",10,25.055962573192524,{"$f":"F2979*(1-Elteq!$F$6)","v":25.055962573192524}]
["ANAMET-S",7824130,"PG 13,5","IEC-Ex ATEX fittings for Sealtite, Adapter PG/NPT nickel plated brass",10,22.789127249551822,{"$f":"F2980*(1-Elteq!$F$6)","v":22.789127249551822}]
["ANAMET-S",7824160,"PG 16","IEC-Ex ATEX fittings for Sealtite, Adapter PG/NPT nickel plated brass",10,22.789127249551822,{"$f":"F2981*(1-Elteq!$F$6)","v":22.789127249551822}]
["ANAMET-S",7824200,"PG 21","IEC-Ex ATEX fittings for Sealtite, Adapter PG/NPT nickel plated brass",5,27.694410244971049,{"$f":"F2982*(1-Elteq!$F$6)","v":27.694410244971049}]
["ANAMET-S",7824260,"PG 29","IEC-Ex ATEX fittings for Sealtite, Adapter PG/NPT nickel plated brass",5,35.033754120692997,{"$f":"F2983*(1-Elteq!$F$6)","v":35.033754120692997}]
["ANAMET-S",7824350,"PG 29","IEC-Ex ATEX fittings for Sealtite, Adapter PG/NPT nickel plated brass",2,38.694135749850524,{"$f":"F2984*(1-Elteq!$F$6)","v":38.694135749850524}]
["ANAMET-S",7824400,"PG 36","IEC-Ex ATEX fittings for Sealtite, Adapter PG/NPT nickel plated brass",1,59.708814037044249,{"$f":"F2985*(1-Elteq!$F$6)","v":59.708814037044249}]
["ANAMET-S",7824500,"PG 48","IEC-Ex ATEX fittings for Sealtite, Adapter PG/NPT nickel plated brass",1,109.03106294363644,{"$f":"F2986*(1-Elteq!$F$6)","v":109.03106294363644}]
["ANAMET-S",7825160,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",10,25.055962573192524,{"$f":"F2987*(1-Elteq!$F$6)","v":25.055962573192524}]
["ANAMET-S",7825200,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",10,22.789127249551822,{"$f":"F2988*(1-Elteq!$F$6)","v":22.789127249551822}]
["ANAMET-S",7825220,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",10,24.57286652061336,{"$f":"F2989*(1-Elteq!$F$6)","v":24.57286652061336}]
["ANAMET-S",7825240,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",5,22.789127249551822,{"$f":"F2990*(1-Elteq!$F$6)","v":22.789127249551822}]
["ANAMET-S",7825250,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",5,24.57286652061336,{"$f":"F2991*(1-Elteq!$F$6)","v":24.57286652061336}]
["ANAMET-S",7825270,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",5,29.589633220473932,{"$f":"F2992*(1-Elteq!$F$6)","v":29.589633220473932}]
["ANAMET-S",7825280,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",5,27.694410244971049,{"$f":"F2993*(1-Elteq!$F$6)","v":27.694410244971049}]
["ANAMET-S",7825320,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",5,29.589633220473932,{"$f":"F2994*(1-Elteq!$F$6)","v":29.589633220473932}]
["ANAMET-S",7825340,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",2,38.694135749850524,{"$f":"F2995*(1-Elteq!$F$6)","v":38.694135749850524}]
["ANAMET-S",7825380,"NPT 1 1/4\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",2,35.033754120692997,{"$f":"F2996*(1-Elteq!$F$6)","v":35.033754120692997}]
["ANAMET-S",7825400,"NPT 1 1/4\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",2,38.694135749850524,{"$f":"F2997*(1-Elteq!$F$6)","v":38.694135749850524}]
["ANAMET-S",7825480,"NPT 1 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",1,48.225992479585614,{"$f":"F2998*(1-Elteq!$F$6)","v":48.225992479585614}]
["ANAMET-S",7825500,"NPT 1 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",1,59.708814037044249,{"$f":"F2999*(1-Elteq!$F$6)","v":59.708814037044249}]
["ANAMET-S",7825520,"NPT 1 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",1,90.115994423421384,{"$f":"F3000*(1-Elteq!$F$6)","v":90.115994423421384}]
["ANAMET-S",7825600,"NPT 2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",2,80.630589237203523,{"$f":"F3001*(1-Elteq!$F$6)","v":80.630589237203523}]
["ANAMET-S",7825630,"NPT 2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/ISO nickel plated brass",1,90.115994423421384,{"$f":"F3002*(1-Elteq!$F$6)","v":90.115994423421384}]
["ANAMET-S",7826120,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/NPT nickel plated brass",10,25.055962573192524,{"$f":"F3003*(1-Elteq!$F$6)","v":25.055962573192524}]
["ANAMET-S",7826160,"M20 x 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/NPT nickel plated brass",10,22.789127249551822,{"$f":"F3004*(1-Elteq!$F$6)","v":22.789127249551822}]
["ANAMET-S",7826180,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/NPT nickel plated brass",10,22.789127249551822,{"$f":"F3005*(1-Elteq!$F$6)","v":22.789127249551822}]
["ANAMET-S",7826200,"M25 x 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/NPT nickel plated brass",5,24.57286652061336,{"$f":"F3006*(1-Elteq!$F$6)","v":24.57286652061336}]
["ANAMET-S",7826260,"M32 x 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/NPT nickel plated brass",5,29.589633220473932,{"$f":"F3007*(1-Elteq!$F$6)","v":29.589633220473932}]
["ANAMET-S",7826350,"M 40 x 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/NPT nickel plated brass",2,35.145237825134338,{"$f":"F3008*(1-Elteq!$F$6)","v":35.145237825134338}]
["ANAMET-S",7826400,"M50 x 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/NPT nickel plated brass",1,59.708814037044249,{"$f":"F3009*(1-Elteq!$F$6)","v":59.708814037044249}]
["ANAMET-S",7826500,"M63 x 1,5","IEC-Ex ATEX fittings for Sealtite, Adapter ISO/NPT nickel plated brass",1,90.115994423421384,{"$f":"F3010*(1-Elteq!$F$6)","v":90.115994423421384}]
["ANAMET-S",7813160,"M 16 x 1,5","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",10,5.7692817048396581,{"$f":"F3011*(1-Elteq!$F$6)","v":5.7692817048396581}]
["ANAMET-S",7813200,"M 20 x 1,5","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",10,6.7354738099979903,{"$f":"F3012*(1-Elteq!$F$6)","v":6.7354738099979903}]
["ANAMET-S",7813250,"M 25 x 1,5","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",5,10.609532539334765,{"$f":"F3013*(1-Elteq!$F$6)","v":10.609532539334765}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},7813320,"M 32 x 1,5","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",5,19.611841672973458,{"$f":"F3014*(1-Elteq!$F$6)","v":19.611841672973458}]
["ANAMET-S",7813400,"M 40 x 1,5","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",2,24.247705715992769,{"$f":"F3015*(1-Elteq!$F$6)","v":24.247705715992769}]
["ANAMET-S",7813500,"M 50 x 1,5","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",1,35.080205664210219,{"$f":"F3016*(1-Elteq!$F$6)","v":35.080205664210219}]
["ANAMET-S",7813630,"M 63 x 1,5","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",1,53.35424288388753,{"$f":"F3017*(1-Elteq!$F$6)","v":53.35424288388753}]
["ANAMET-S",7813750,"M 75 x 1,5","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",1,87.793417247560015,{"$f":"F3018*(1-Elteq!$F$6)","v":87.793417247560015}]
["ANAMET-S",7814160,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",10,9.0487606771559221,{"$f":"F3019*(1-Elteq!$F$6)","v":9.0487606771559221}]
["ANAMET-S",7814200,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",10,11.371337853017296,{"$f":"F3020*(1-Elteq!$F$6)","v":11.371337853017296}]
["ANAMET-S",7814260,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",5,19.342422720573538,{"$f":"F3021*(1-Elteq!$F$6)","v":19.342422720573538}]
["ANAMET-S",7814350,"NPT 1.1/4\"","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",2,27.480733144791802,{"$f":"F3022*(1-Elteq!$F$6)","v":27.480733144791802}]
["ANAMET-S",7814400,"NPT 1.1/2\"","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",1,38.36897494522993,{"$f":"F3023*(1-Elteq!$F$6)","v":38.36897494522993}]
["ANAMET-S",7814500,"NPT 2\"","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",1,53.35424288388753,{"$f":"F3024*(1-Elteq!$F$6)","v":53.35424288388753}]
["ANAMET-S",7815110,"PG 11","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",10,7.1070861581358109,{"$f":"F3025*(1-Elteq!$F$6)","v":7.1070861581358109}]
["ANAMET-S",7815130,"PG 13,5","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",10,9.0487606771559221,{"$f":"F3026*(1-Elteq!$F$6)","v":9.0487606771559221}]
["ANAMET-S",7815160,"PG 16","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",10,11.371337853017296,{"$f":"F3027*(1-Elteq!$F$6)","v":11.371337853017296}]
["ANAMET-S",7815210,"PG 21","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",5,19.342422720573538,{"$f":"F3028*(1-Elteq!$F$6)","v":19.342422720573538}]
["ANAMET-S",7815290,"PG 29","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",5,27.480733144791802,{"$f":"F3029*(1-Elteq!$F$6)","v":27.480733144791802}]
["ANAMET-S",7815360,"PG 36","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",2,38.36897494522993,{"$f":"F3030*(1-Elteq!$F$6)","v":38.36897494522993}]
["ANAMET-S",7815480,"PG 48","IEC-Ex ATEX fittings for Sealtite, Blindplug nickel plated brass",1,87.793417247560015,{"$f":"F3031*(1-Elteq!$F$6)","v":87.793417247560015}]
["ANAMET-S",7817160,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/NPT male nickel plated brass",10,22.789127249551822,{"$f":"F3032*(1-Elteq!$F$6)","v":22.789127249551822}]
["ANAMET-S",7817200,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/NPT male nickel plated brass",5,24.57286652061336,{"$f":"F3033*(1-Elteq!$F$6)","v":24.57286652061336}]
["ANAMET-S",7817260,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/NPT male nickel plated brass",5,29.589633220473932,{"$f":"F3034*(1-Elteq!$F$6)","v":29.589633220473932}]
["ANAMET-S",7817350,"NPT 1 1/4\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/NPT male nickel plated brass",2,38.694135749850524,{"$f":"F3035*(1-Elteq!$F$6)","v":38.694135749850524}]
["ANAMET-S",7817400,"NPT 1 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/NPT male nickel plated brass",1,59.708814037044249,{"$f":"F3036*(1-Elteq!$F$6)","v":59.708814037044249}]
["ANAMET-S",7817500,"NPT 2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/NPT male nickel plated brass",1,90.115994423421384,{"$f":"F3037*(1-Elteq!$F$6)","v":90.115994423421384}]
["ANAMET-S",7823110,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/PG nickel plated brass",10,25.055962573192524,{"$f":"F3038*(1-Elteq!$F$6)","v":25.055962573192524}]
["ANAMET-S",7823130,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/PG nickel plated brass",10,25.055962573192524,{"$f":"F3039*(1-Elteq!$F$6)","v":25.055962573192524}]
["ANAMET-S",7823160,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/PG nickel plated brass",10,24.57286652061336,{"$f":"F3040*(1-Elteq!$F$6)","v":24.57286652061336}]
["ANAMET-S",7823200,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/PG nickel plated brass",10,24.57286652061336,{"$f":"F3041*(1-Elteq!$F$6)","v":24.57286652061336}]
["ANAMET-S",7823210,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/PG nickel plated brass",5,29.589633220473932,{"$f":"F3042*(1-Elteq!$F$6)","v":29.589633220473932}]
["ANAMET-S",7823260,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/PG nickel plated brass",5,29.589633220473932,{"$f":"F3043*(1-Elteq!$F$6)","v":29.589633220473932}]
["ANAMET-S",7823290,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/PG nickel plated brass",5,38.694135749850524,{"$f":"F3044*(1-Elteq!$F$6)","v":38.694135749850524}]
["ANAMET-S",7823300,"NPT 1 1/4\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/PG nickel plated brass",2,38.694135749850524,{"$f":"F3045*(1-Elteq!$F$6)","v":38.694135749850524}]
["ANAMET-S",7823360,"NPT 1 1/4\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/PG nickel plated brass",1,59.708814037044249,{"$f":"F3046*(1-Elteq!$F$6)","v":59.708814037044249}]
["ANAMET-S",7823400,"NPT 1 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/PG nickel plated brass",1,59.708814037044249,{"$f":"F3047*(1-Elteq!$F$6)","v":59.708814037044249}]
["ANAMET-S",7823420,"NPT 1 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/PG nickel plated brass",1,90.115994423421384,{"$f":"F3048*(1-Elteq!$F$6)","v":90.115994423421384}]
["ANAMET-S",7823480,"NPT 2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/PG nickel plated brass",1,127.67671251145158,{"$f":"F3049*(1-Elteq!$F$6)","v":127.67671251145158}]
["ANAMET-S",7827160,"NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/NPT fem nickel plated brass",10,22.789127249551822,{"$f":"F3050*(1-Elteq!$F$6)","v":22.789127249551822}]
["ANAMET-S",7827200,"NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/NPT fem nickel plated brass",5,24.57286652061336,{"$f":"F3051*(1-Elteq!$F$6)","v":24.57286652061336}]
["ANAMET-S",7827260,"NPT 1\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/NPT fem nickel plated brass",5,29.589633220473932,{"$f":"F3052*(1-Elteq!$F$6)","v":29.589633220473932}]
["ANAMET-S",7827350,"NPT 1 1/4\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/NPT fem nickel plated brass",2,38.694135749850524,{"$f":"F3053*(1-Elteq!$F$6)","v":38.694135749850524}]
["ANAMET-S",7827400,"NPT 1 1/2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/NPT fem nickel plated brass",1,59.708814037044249,{"$f":"F3054*(1-Elteq!$F$6)","v":59.708814037044249}]
["ANAMET-S",7827500,"NPT 2\"","IEC-Ex ATEX fittings for Sealtite, Adapter NPT/NPT fem nickel plated brass",1,90.115994423421384,{"$f":"F3055*(1-Elteq!$F$6)","v":90.115994423421384}]
["ANAMET-S",7829160,"M16 x 1,5","IEC-Ex ATEX fittings for Sealtite, Fitting dus cap EPDM",10,5.9086363353913409,{"$f":"F3056*(1-Elteq!$F$6)","v":5.9086363353913409}]
["ANAMET-S",7829200,"M20 x 1,5 / NPT 1/2\"","IEC-Ex ATEX fittings for Sealtite, Fitting dus cap EPDM",10,6.2802486835291607,{"$f":"F3057*(1-Elteq!$F$6)","v":6.2802486835291607}]
["ANAMET-S",7829250,"M25 x 1,5 / NPT 3/4\"","IEC-Ex ATEX fittings for Sealtite, Fitting dus cap EPDM",5,6.8097962796255542,{"$f":"F3058*(1-Elteq!$F$6)","v":6.8097962796255542}]
["ANAMET-S",7829320,"M32 x 1,5 / NPT 1\"","IEC-Ex ATEX fittings for Sealtite, Fitting dus cap EPDM",5,8.6399870942043204,{"$f":"F3059*(1-Elteq!$F$6)","v":8.6399870942043204}]
["ANAMET-S",7829400,"M40 x 1,5 / NPT 1.1/4\"","IEC-Ex ATEX fittings for Sealtite, Fitting dus cap EPDM",2,11.464240940051752,{"$f":"F3060*(1-Elteq!$F$6)","v":11.464240940051752}]
["ANAMET-S",7829500,"M50 x 1,5 / NPT 1.1/2\"","IEC-Ex ATEX fittings for Sealtite, Fitting dus cap EPDM",2,14.399978490340532,{"$f":"F3061*(1-Elteq!$F$6)","v":14.399978490340532}]
["ANAMET-S",7829630,"M63 x 1,5 / NPT 2\"","IEC-Ex ATEX fittings for Sealtite, Fitting dus cap EPDM",2,16.546039800836443,{"$f":"F3062*(1-Elteq!$F$6)","v":16.546039800836443}]
["ANAMET-S",8279991,"50 gr","IEC-Ex ATEX fittings for Sealtite, Sealing compound for BXA/BXC/BXN",10,7.7574077673769963,{"$f":"F3063*(1-Elteq!$F$6)","v":7.7574077673769963}]
["ANAMET-S",8801168,"M16 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 316",50,14.121269229237166,{"$f":"F3064*(1-Elteq!$F$6)","v":14.121269229237166}]
["ANAMET-S",8801208,"M20 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 316",50,16.258040231029632,{"$f":"F3065*(1-Elteq!$F$6)","v":16.258040231029632}]
["ANAMET-S",8801258,"M25 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 316",25,19.46319673371833,{"$f":"F3066*(1-Elteq!$F$6)","v":19.46319673371833}]
["ANAMET-S",8801328,"M32 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 316",20,34.699303007368961,{"$f":"F3067*(1-Elteq!$F$6)","v":34.699303007368961}]
["ANAMET-S",8801408,"M40 x 1,5","Fitting accessories for Sealtite, Locknut, stainless steel 316",10,47.752186735709884,{"$f":"F3068*(1-Elteq!$F$6)","v":47.752186735709884}]
["ANAMET-S",8802168,"NPT 1/2\"","Fitting accessories for Sealtite, Locknut, stainless steel 316",50,17.326425731925863,{"$f":"F3069*(1-Elteq!$F$6)","v":17.326425731925863}]
["ANAMET-S",8802208,"NPT 3/4\"","Fitting accessories for Sealtite, Locknut, stainless steel 316",50,20.578033778131793,{"$f":"F3070*(1-Elteq!$F$6)","v":20.578033778131793}]
["ANAMET-S",8802268,"NPT 1\"","Fitting accessories for Sealtite, Locknut, stainless steel 316",20,36.836074009161422,{"$f":"F3071*(1-Elteq!$F$6)","v":36.836074009161422}]
["ANAMET-S",8802358,"NPT 1.1/4\"","Fitting accessories for Sealtite, Locknut, stainless steel 316",10,49.888957737502359,{"$f":"F3072*(1-Elteq!$F$6)","v":49.888957737502359}]
["ANAMET-S",8802408,"NPT 1.1/2\"","Fitting accessories for Sealtite, Locknut, stainless steel 316",5,81.290201155148168,{"$f":"F3073*(1-Elteq!$F$6)","v":81.290201155148168}]
["ANAMET-S",3130121,"3/8\"","CNP conduit with grey cover, Full plastic, nylon reinfored, IP 67",76,12.839206628161687,{"$f":"F3074*(1-Elteq!$F$6)","v":12.839206628161687}]
["ANAMET-S",3130161,"1/2\"","CNP conduit with grey cover, Full plastic, nylon reinfored, IP 67",60,16.555330109539888,{"$f":"F3075*(1-Elteq!$F$6)","v":16.555330109539888}]
["ANAMET-S",3130201,"3/4\"","CNP conduit with grey cover, Full plastic, nylon reinfored, IP 67",53,23.597384106751576,{"$f":"F3076*(1-Elteq!$F$6)","v":23.597384106751576}]
["ANAMET-S",3130261,"1\"","CNP conduit with grey cover, Full plastic, nylon reinfored, IP 67",30,29.431697972515355,{"$f":"F3077*(1-Elteq!$F$6)","v":29.431697972515355}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},3130351,"1 1/4\"","CNP conduit with grey cover, Full plastic, nylon reinfored, IP 67",15,39.446650754829612,{"$f":"F3078*(1-Elteq!$F$6)","v":39.446650754829612}]
["ANAMET-S",3130401,"1 1/2\"","CNP conduit with grey cover, Full plastic, nylon reinfored, IP 67",15,62.728164365664043,{"$f":"F3079*(1-Elteq!$F$6)","v":62.728164365664043}]
["ANAMET-S",3130501,"2\"","CNP conduit with grey cover, Full plastic, nylon reinfored, IP 67",15,87.681933543118674,{"$f":"F3080*(1-Elteq!$F$6)","v":87.681933543118674}]
["ANAMET-S",3210121,"3/8\"","CNP conduit with orange cover, Full plastic, nylon reinfored, IP 67",76,12.839206628161687,{"$f":"F3081*(1-Elteq!$F$6)","v":12.839206628161687}]
["ANAMET-S",3210161,"1/2\"","CNP conduit with orange cover, Full plastic, nylon reinfored, IP 67",60,16.555330109539888,{"$f":"F3082*(1-Elteq!$F$6)","v":16.555330109539888}]
["ANAMET-S",3210201,"3/4\"","CNP conduit with orange cover, Full plastic, nylon reinfored, IP 67",53,23.597384106751576,{"$f":"F3083*(1-Elteq!$F$6)","v":23.597384106751576}]
["ANAMET-S",3210261,"1\"","CNP conduit with orange cover, Full plastic, nylon reinfored, IP 67",30,29.431697972515355,{"$f":"F3084*(1-Elteq!$F$6)","v":29.431697972515355}]
["ANAMET-S",3210351,"1 1/4\"","CNP conduit with orange cover, Full plastic, nylon reinfored, IP 67",15,39.446650754829612,{"$f":"F3085*(1-Elteq!$F$6)","v":39.446650754829612}]
["ANAMET-S",3210401,"1 1/2\"","CNP conduit with orange cover, Full plastic, nylon reinfored, IP 67",15,62.728164365664043,{"$f":"F3086*(1-Elteq!$F$6)","v":62.728164365664043}]
["ANAMET-S",3210501,"2\"","CNP conduit with orange cover, Full plastic, nylon reinfored, IP 67",15,87.681933543118674,{"$f":"F3087*(1-Elteq!$F$6)","v":87.681933543118674}]
["ANAMET-S",2983120,"NPT 1/2\"","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",25,15.812105413264247,{"$f":"F3088*(1-Elteq!$F$6)","v":15.812105413264247}]
["ANAMET-S",2983160,"NPT 1/2\"","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",25,17.976747341167052,{"$f":"F3089*(1-Elteq!$F$6)","v":17.976747341167052}]
["ANAMET-S",2983200,"NPT 3/4\"","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",25,24.842285473013277,{"$f":"F3090*(1-Elteq!$F$6)","v":24.842285473013277}]
["ANAMET-S",2983260,"NPT 1\"","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",5,38.629103588926405,{"$f":"F3091*(1-Elteq!$F$6)","v":38.629103588926405}]
["ANAMET-S",2983350,"NPT 1 1/4\"","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",5,58.138751866161968,{"$f":"F3092*(1-Elteq!$F$6)","v":58.138751866161968}]
["ANAMET-S",2983400,"NPT 1 1/2\"","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",2,109.62564270065695,{"$f":"F3093*(1-Elteq!$F$6)","v":109.62564270065695}]
["ANAMET-S",2983500,"2\"","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",1,154.7393817645883,{"$f":"F3094*(1-Elteq!$F$6)","v":154.7393817645883}]
["ANAMET-S",2987120,"NPT 1/2\"","Sealtite fittings for CNP, 90° elbow fixed with male thread, IP 67",25,29.450278589922249,{"$f":"F3095*(1-Elteq!$F$6)","v":29.450278589922249}]
["ANAMET-S",2987160,"NPT 1/2\"","Sealtite fittings for CNP, 90° elbow fixed with male thread, IP 67",25,29.450278589922249,{"$f":"F3096*(1-Elteq!$F$6)","v":29.450278589922249}]
["ANAMET-S",2987200,"NPT 3/4\"","Sealtite fittings for CNP, 90° elbow fixed with male thread, IP 67",25,44.779287950607333,{"$f":"F3097*(1-Elteq!$F$6)","v":44.779287950607333}]
["ANAMET-S",2987260,"NPT 1\"","Sealtite fittings for CNP, 90° elbow fixed with male thread, IP 67",5,83.20400474805794,{"$f":"F3098*(1-Elteq!$F$6)","v":83.20400474805794}]
["ANAMET-S",2987350,"NPT 1 1/4\"","Sealtite fittings for CNP, 90° elbow fixed with male thread, IP 67",5,138.3234062856001,{"$f":"F3099*(1-Elteq!$F$6)","v":138.3234062856001}]
["ANAMET-S",2987400,"NPT 1 1/2\"","Sealtite fittings for CNP, 90° elbow fixed with male thread, IP 67",2,212.98032702648817,{"$f":"F3100*(1-Elteq!$F$6)","v":212.98032702648817}]
["ANAMET-S",2987500,"NPT 2\"","Sealtite fittings for CNP, 90° elbow fixed with male thread, IP 67",1,261.55935123680479,{"$f":"F3101*(1-Elteq!$F$6)","v":261.55935123680479}]
["ANAMET-S",8280169,"M 16 x 1,5","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",10,39.400199211312376,{"$f":"F3102*(1-Elteq!$F$6)","v":39.400199211312376}]
["ANAMET-S",8280209,"M 20 x 1,5","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",10,50.548569655446983,{"$f":"F3103*(1-Elteq!$F$6)","v":50.548569655446983}]
["ANAMET-S",8280259,"M 25 x 1,5","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",5,55.082240302728394,{"$f":"F3104*(1-Elteq!$F$6)","v":55.082240302728394}]
["ANAMET-S",8280329,"M 32 x 1,5","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",5,86.752902672774113,{"$f":"F3105*(1-Elteq!$F$6)","v":86.752902672774113}]
["ANAMET-S",8280409,"M 40 x 1,5","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",2,109.93222288787064,{"$f":"F3106*(1-Elteq!$F$6)","v":109.93222288787064}]
["ANAMET-S",8280509,"M 50 x 1,5","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",2,153.31796453296116,{"$f":"F3107*(1-Elteq!$F$6)","v":153.31796453296116}]
["ANAMET-S",8280609,"M 63 x 1,5","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",2,185.54604542521361,{"$f":"F3108*(1-Elteq!$F$6)","v":185.54604542521361}]
["ANAMET-S",8280639,"M 63 x 1,5","Sealtite fittings for CNP, Straight fixed with male thread, IP 67",2,218.00638403505221,{"$f":"F3109*(1-Elteq!$F$6)","v":218.00638403505221}]
["ANAMET-S",3000120,"3/8\"","NMUA conduit with grey cover, Full plastic, pvc reinfored, IP 67",30,3.502446381198955,{"$f":"F3110*(1-Elteq!$F$6)","v":3.502446381198955}]
["ANAMET-S",3000160,"1/2\"","NMUA conduit with grey cover, Full plastic, pvc reinfored, IP 67",30,3.7532847161919838,{"$f":"F3111*(1-Elteq!$F$6)","v":3.7532847161919838}]
["ANAMET-S",3000200,"3/4\"","NMUA conduit with grey cover, Full plastic, pvc reinfored, IP 67",30,4.4407675602469512,{"$f":"F3112*(1-Elteq!$F$6)","v":4.4407675602469512}]
["ANAMET-S",3000260,"1\"","NMUA conduit with grey cover, Full plastic, pvc reinfored, IP 67",30,7.162828010356483,{"$f":"F3113*(1-Elteq!$F$6)","v":7.162828010356483}]
["ANAMET-S",3000350,"1 1/4\"","NMUA conduit with grey cover, Full plastic, pvc reinfored, IP 67",15,8.8257932682732285,{"$f":"F3114*(1-Elteq!$F$6)","v":8.8257932682732285}]
["ANAMET-S",3000400,"1 1/2\"","NMUA conduit with grey cover, Full plastic, pvc reinfored, IP 67",15,11.557144027086206,{"$f":"F3115*(1-Elteq!$F$6)","v":11.557144027086206}]
["ANAMET-S",3000500,"2\"","NMUA conduit with grey cover, Full plastic, pvc reinfored, IP 67",15,15.997911587333157,{"$f":"F3116*(1-Elteq!$F$6)","v":15.997911587333157}]
["ANAMET-S",3250120,"3/8\"","NMSF conduit with grey cover, Full plastic, pvc reinfored, IP 67",30,2.3597384106751584,{"$f":"F3117*(1-Elteq!$F$6)","v":2.3597384106751584}]
["ANAMET-S",3250160,"1/2\"","NMSF conduit with grey cover, Full plastic, pvc reinfored, IP 67",30,2.39689964548894,{"$f":"F3118*(1-Elteq!$F$6)","v":2.39689964548894}]
["ANAMET-S",3250200,"3/4\"","NMSF conduit with grey cover, Full plastic, pvc reinfored, IP 67",30,3.1308340330611348,{"$f":"F3119*(1-Elteq!$F$6)","v":3.1308340330611348}]
["ANAMET-S",3250260,"1\"","NMSF conduit with grey cover, Full plastic, pvc reinfored, IP 67",30,4.4872191037641791,{"$f":"F3120*(1-Elteq!$F$6)","v":4.4872191037641791}]
["ANAMET-S",3250350,"1 1/4\"","NMSF conduit with grey cover, Full plastic, pvc reinfored, IP 67",15,6.4846354750049624,{"$f":"F3121*(1-Elteq!$F$6)","v":6.4846354750049624}]
["ANAMET-S",3250400,"1 1/2\"","NMSF conduit with grey cover, Full plastic, pvc reinfored, IP 67",15,8.5935355506870899,{"$f":"F3122*(1-Elteq!$F$6)","v":8.5935355506870899}]
["ANAMET-S",3250500,"2\"","NMSF conduit with grey cover, Full plastic, pvc reinfored, IP 67",15,12.003078844851592,{"$f":"F3123*(1-Elteq!$F$6)","v":12.003078844851592}]
["ANAMET-S",2630160,"M16 x 1,5","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",25,2.0903194582752387,{"$f":"F3124*(1-Elteq!$F$6)","v":2.0903194582752387}]
["ANAMET-S",2630200,"M20 x 1,5","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",25,2.0903194582752387,{"$f":"F3125*(1-Elteq!$F$6)","v":2.0903194582752387}]
["ANAMET-S",2630250,"M25 x 1,5","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",10,2.5083833499302863,{"$f":"F3126*(1-Elteq!$F$6)","v":2.5083833499302863}]
["ANAMET-S",2630320,"M32 x 1,5","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",5,3.9019296554471117,{"$f":"F3127*(1-Elteq!$F$6)","v":3.9019296554471117}]
["ANAMET-S",2631160,"M16 x 1,5","Sealtite fittings for NMUA/NMSF, 90° elbow fixed with male thread, IP 67",25,2.415480262895831,{"$f":"F3128*(1-Elteq!$F$6)","v":2.415480262895831}]
["ANAMET-S",2631200,"M20 x 1,5","Sealtite fittings for NMUA/NMSF, 90° elbow fixed with male thread, IP 67",25,2.415480262895831,{"$f":"F3129*(1-Elteq!$F$6)","v":2.415480262895831}]
["ANAMET-S",2631250,"M25 x 1,5","Sealtite fittings for NMUA/NMSF, 90° elbow fixed with male thread, IP 67",10,2.7685119936267601,{"$f":"F3130*(1-Elteq!$F$6)","v":2.7685119936267601}]
["ANAMET-S",2631320,"M32 x 1,5","Sealtite fittings for NMUA/NMSF, 90° elbow fixed with male thread, IP 67",5,4.0412842859987936,{"$f":"F3131*(1-Elteq!$F$6)","v":4.0412842859987936}]
["ANAMET-S",2633120,"NPT 1/2\"","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",25,2.0903194582752387,{"$f":"F3132*(1-Elteq!$F$6)","v":2.0903194582752387}]
["ANAMET-S",2633160,"NPT 1/2\"","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",25,2.0903194582752387,{"$f":"F3133*(1-Elteq!$F$6)","v":2.0903194582752387}]
["ANAMET-S",2633200,"NPT 3/4\"","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",10,2.5083833499302863,{"$f":"F3134*(1-Elteq!$F$6)","v":2.5083833499302863}]
["ANAMET-S",2633260,"NPT 1","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",5,3.9019296554471117,{"$f":"F3135*(1-Elteq!$F$6)","v":3.9019296554471117}]
["ANAMET-S",2633350,"NPT 1.1/4","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",5,4.645154351722752,{"$f":"F3136*(1-Elteq!$F$6)","v":4.645154351722752}]
["ANAMET-S",2633400,"NPT 1.1/2","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",2,5.8993460266878941,{"$f":"F3137*(1-Elteq!$F$6)","v":5.8993460266878941}]
["ANAMET-S",2633500,"NPT 2","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",2,8.7793417247560015,{"$f":"F3138*(1-Elteq!$F$6)","v":8.7793417247560015}]
["ANAMET-S",2634120,"NPT 1/2\"","Sealtite fittings for NMUA/NMSF, 90° elbow fixed with male thread, IP 67",25,2.415480262895831,{"$f":"F3139*(1-Elteq!$F$6)","v":2.415480262895831}]
["ANAMET-S",2634160,"NPT 1/2\"","Sealtite fittings for NMUA/NMSF, 90° elbow fixed with male thread, IP 67",25,2.415480262895831,{"$f":"F3140*(1-Elteq!$F$6)","v":2.415480262895831}]
["ANAMET-S",2634200,"NPT 3/4\"","Sealtite fittings for NMUA/NMSF, 90° elbow fixed with male thread, IP 67",10,2.7685119936267601,{"$f":"F3141*(1-Elteq!$F$6)","v":2.7685119936267601}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},2634260,"NPT 1","Sealtite fittings for NMUA/NMSF, 90° elbow fixed with male thread, IP 67",5,4.0412842859987936,{"$f":"F3142*(1-Elteq!$F$6)","v":4.0412842859987936}]
["ANAMET-S",2634350,"NPT 1.1/4","Sealtite fittings for NMUA/NMSF, 90° elbow fixed with male thread, IP 67",5,7.1535377016530379,{"$f":"F3143*(1-Elteq!$F$6)","v":7.1535377016530379}]
["ANAMET-S",2634400,"NPT 1.1/2","Sealtite fittings for NMUA/NMSF, 90° elbow fixed with male thread, IP 67",2,9.271728086038614,{"$f":"F3144*(1-Elteq!$F$6)","v":9.271728086038614}]
["ANAMET-S",2634500,"NPT 2","Sealtite fittings for NMUA/NMSF, 90° elbow fixed with male thread, IP 67",2,14.074817685719939,{"$f":"F3145*(1-Elteq!$F$6)","v":14.074817685719939}]
["ANAMET-S",8100101,"PG 9","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,3.9669618163712301,{"$f":"F3146*(1-Elteq!$F$6)","v":3.9669618163712301}]
["ANAMET-S",8100111,"PG 11","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,4.0784455208125756,{"$f":"F3147*(1-Elteq!$F$6)","v":4.0784455208125756}]
["ANAMET-S",8100131,"PG 13,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,4.0784455208125756,{"$f":"F3148*(1-Elteq!$F$6)","v":4.0784455208125756}]
["ANAMET-S",8100161,"PG 16","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,4.756638056164098,{"$f":"F3149*(1-Elteq!$F$6)","v":4.756638056164098}]
["ANAMET-S",8100210,"M25 x 1,5","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",5,10.163597721569381,{"$f":"F3150*(1-Elteq!$F$6)","v":10.163597721569381}]
["ANAMET-S",8100211,"PG 21","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",5,6.2988293009360516,{"$f":"F3151*(1-Elteq!$F$6)","v":6.2988293009360516}]
["ANAMET-S",8100291,"PG 29","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",5,10.888241800438133,{"$f":"F3152*(1-Elteq!$F$6)","v":10.888241800438133}]
["ANAMET-S",8100361,"PG 36","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",2,17.846683019318814,{"$f":"F3153*(1-Elteq!$F$6)","v":17.846683019318814}]
["ANAMET-S",8100421,"PG 42","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",2,23.95041583748251,{"$f":"F3154*(1-Elteq!$F$6)","v":23.95041583748251}]
["ANAMET-S",8100481,"PG 48","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",2,36.724590304720074,{"$f":"F3155*(1-Elteq!$F$6)","v":36.724590304720074}]
["ANAMET-S",8120161,"M16 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,3.8183168771161027,{"$f":"F3156*(1-Elteq!$F$6)","v":3.8183168771161027}]
["ANAMET-S",8120171,"M20 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,4.1063164469229125,{"$f":"F3157*(1-Elteq!$F$6)","v":4.1063164469229125}]
["ANAMET-S",8120201,"M20 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",10,4.1063164469229125,{"$f":"F3158*(1-Elteq!$F$6)","v":4.1063164469229125}]
["ANAMET-S",8120250,"M25 x 1,5","Sealtite fittings for NMUA/NMSF, Straight fixed with male thread, IP 67",5,6.3452808444532796,{"$f":"F3159*(1-Elteq!$F$6)","v":6.3452808444532796}]
["ANAMET-S",8120321,"M32 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",5,9.7455338299143328,{"$f":"F3160*(1-Elteq!$F$6)","v":9.7455338299143328}]
["ANAMET-S",8120401,"M40 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",2,17.846683019318814,{"$f":"F3161*(1-Elteq!$F$6)","v":17.846683019318814}]
["ANAMET-S",8120501,"M50 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",2,23.95041583748251,{"$f":"F3162*(1-Elteq!$F$6)","v":23.95041583748251}]
["ANAMET-S",8120631,"M63 x 1,5","Standard fittings for Sealtite, Straight fixed with male thread, IP 67",2,36.724590304720074,{"$f":"F3163*(1-Elteq!$F$6)","v":36.724590304720074}]
["ANAMET-S",3590120,"3/8\"","NMFG conduit with blue cover, Full plastic, pvc reinfored, IP 67",30,6.9305702927703461,{"$f":"F3164*(1-Elteq!$F$6)","v":6.9305702927703461}]
["ANAMET-S",3590160,"1/2\"","NMFG conduit with blue cover, Full plastic, pvc reinfored, IP 67",30,6.9305702927703461,{"$f":"F3165*(1-Elteq!$F$6)","v":6.9305702927703461}]
["ANAMET-S",3590200,"3/4\"","NMFG conduit with blue cover, Full plastic, pvc reinfored, IP 67",30,8.6306967855008718,{"$f":"F3166*(1-Elteq!$F$6)","v":8.6306967855008718}]
["ANAMET-S",3590260,"1\"","NMFG conduit with blue cover, Full plastic, pvc reinfored, IP 67",30,12.142433475403275,{"$f":"F3167*(1-Elteq!$F$6)","v":12.142433475403275}]
["ANAMET-S",3590350,"1 1/4\"","NMFG conduit with blue cover, Full plastic, pvc reinfored, IP 67",15,13.805398733320018,{"$f":"F3168*(1-Elteq!$F$6)","v":13.805398733320018}]
["ANAMET-S",3590400,"1 1/2\"","NMFG conduit with blue cover, Full plastic, pvc reinfored, IP 67",15,19.13803592909774,{"$f":"F3169*(1-Elteq!$F$6)","v":19.13803592909774}]
["ANAMET-S",3590500,"2\"","NMFG conduit with blue cover, Full plastic, pvc reinfored, IP 67",15,26.495960422226577,{"$f":"F3170*(1-Elteq!$F$6)","v":26.495960422226577}]
["ANAMET-S",7189400,"M40 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",2,37.374911913961263,{"$f":"F3171*(1-Elteq!$F$6)","v":37.374911913961263}]
["ANAMET-S",7189500,"M50 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",2,50.372053790081523,{"$f":"F3172*(1-Elteq!$F$6)","v":50.372053790081523}]
["ANAMET-S",7189630,"M63 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",2,75.613822537342955,{"$f":"F3173*(1-Elteq!$F$6)","v":75.613822537342955}]
["ANAMET-S",8189161,"M16 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",10,13.470947619995981,{"$f":"F3174*(1-Elteq!$F$6)","v":13.470947619995981}]
["ANAMET-S",8189201,"M20 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",10,17.18707110137418,{"$f":"F3175*(1-Elteq!$F$6)","v":17.18707110137418}]
["ANAMET-S",8189251,"M25 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",5,21.739322366062478,{"$f":"F3176*(1-Elteq!$F$6)","v":21.739322366062478}]
["ANAMET-S",8189321,"M32 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",5,37.904459510057656,{"$f":"F3177*(1-Elteq!$F$6)","v":37.904459510057656}]
["ANAMET-S",8189401,"M40 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",2,62.709583748257153,{"$f":"F3178*(1-Elteq!$F$6)","v":62.709583748257153}]
["ANAMET-S",8189501,"M50 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",2,81.290201155148168,{"$f":"F3179*(1-Elteq!$F$6)","v":81.290201155148168}]
["ANAMET-S",8189631,"M63 x 1,5","Food grade fittings for Sealtite, 90° elbow Polished male thread, IP 67",2,127.2772292372034,{"$f":"F3180*(1-Elteq!$F$6)","v":127.2772292372034}]
["ANAMET-S",8320169,"M 16 x 1,5","Food grade fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",10,40.951680764787774,{"$f":"F3181*(1-Elteq!$F$6)","v":40.951680764787774}]
["ANAMET-S",8320209,"M 20 x 1,5","Food grade fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",10,40.951680764787774,{"$f":"F3182*(1-Elteq!$F$6)","v":40.951680764787774}]
["ANAMET-S",8320259,"M 25 x 1,5","Food grade fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",5,55.39811079864554,{"$f":"F3183*(1-Elteq!$F$6)","v":55.39811079864554}]
["ANAMET-S",8320329,"M 32 x 1,5","Food grade fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",5,81.949813073092784,{"$f":"F3184*(1-Elteq!$F$6)","v":81.949813073092784}]
["ANAMET-S",8320409,"M 40 x 1,5","Food grade fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",2,118.57220998207495,{"$f":"F3185*(1-Elteq!$F$6)","v":118.57220998207495}]
["ANAMET-S",8320509,"M 50 x 1,5","Food grade fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",2,186.07559302131,{"$f":"F3186*(1-Elteq!$F$6)","v":186.07559302131}]
["ANAMET-S",8320639,"M 63 x 1,5","Food grade fittings for Sealtite, Stainless steel 316 Straight fixed IP 67",1,415.55550830511743,{"$f":"F3187*(1-Elteq!$F$6)","v":415.55550830511743}]
["ANAMET-S",6203090,"MPC","MPC conduit with grey cover, Full plastic, metal reinfored, IP 67",50,3.8647684206333297,{"$f":"F3188*(1-Elteq!$F$6)","v":3.8647684206333297}]
["ANAMET-S",6203091,"MPC","MPC conduit with grey cover, Full plastic, metal reinfored, IP 67",10,4.2549613861780404,{"$f":"F3189*(1-Elteq!$F$6)","v":4.2549613861780404}]
["ANAMET-S",6203110,"MPC","MPC conduit with grey cover, Full plastic, metal reinfored, IP 67",50,4.4128966341366143,{"$f":"F3190*(1-Elteq!$F$6)","v":4.4128966341366143}]
["ANAMET-S",6203111,"MPC","MPC conduit with grey cover, Full plastic, metal reinfored, IP 67",10,4.8588314519019988,{"$f":"F3191*(1-Elteq!$F$6)","v":4.8588314519019988}]
["ANAMET-S",6203130,"MPC","MPC conduit with grey cover, Full plastic, metal reinfored, IP 67",50,5.0260570085640177,{"$f":"F3192*(1-Elteq!$F$6)","v":5.0260570085640177}]
["ANAMET-S",6203131,"MPC","MPC conduit with grey cover, Full plastic, metal reinfored, IP 67",10,5.5277336785500752,{"$f":"F3193*(1-Elteq!$F$6)","v":5.5277336785500752}]
["ANAMET-S",6203160,"MPC","MPC conduit with grey cover, Full plastic, metal reinfored, IP 67",50,5.4905724437362924,{"$f":"F3194*(1-Elteq!$F$6)","v":5.4905724437362924}]
["ANAMET-S",6203161,"MPC","MPC conduit with grey cover, Full plastic, metal reinfored, IP 67",10,6.0201200398326877,{"$f":"F3195*(1-Elteq!$F$6)","v":6.0201200398326877}]
["ANAMET-S",6203210,"MPC","MPC conduit with grey cover, Full plastic, metal reinfored, IP 67",50,5.8993460266878941,{"$f":"F3196*(1-Elteq!$F$6)","v":5.8993460266878941}]
["ANAMET-S",6203211,"MPC","MPC conduit with grey cover, Full plastic, metal reinfored, IP 67",10,6.4753451663015156,{"$f":"F3197*(1-Elteq!$F$6)","v":6.4753451663015156}]
["ANAMET-S",6203290,"MPC","MPC conduit with grey cover, Full plastic, metal reinfored, IP 67",25,8.9094060466042393,{"$f":"F3198*(1-Elteq!$F$6)","v":8.9094060466042393}]
["ANAMET-S",6203291,"MPC","MPC conduit with grey cover, Full plastic, metal reinfored, IP 67",10,9.8105659908384535,{"$f":"F3199*(1-Elteq!$F$6)","v":9.8105659908384535}]
["ANAMET-S",6203360,"MPC","MPC conduit with grey cover, Full plastic, metal reinfored, IP 67",25,12.737013232423786,{"$f":"F3200*(1-Elteq!$F$6)","v":12.737013232423786}]
["ANAMET-S",6203361,"MPC","MPC conduit with grey cover, Full plastic, metal reinfored, IP 67",10,14.019075833499265,{"$f":"F3201*(1-Elteq!$F$6)","v":14.019075833499265}]
["ANAMET-S",6203420,"MPC","MPC conduit with grey cover, Full plastic, metal reinfored, IP 67",25,16.499588257319218,{"$f":"F3202*(1-Elteq!$F$6)","v":16.499588257319218}]
["ANAMET-S",6203421,"MPC","MPC conduit with grey cover, Full plastic, metal reinfored, IP 67",10,18.14397289782907,{"$f":"F3203*(1-Elteq!$F$6)","v":18.14397289782907}]
["ANAMET-S",6203480,"MPC","MPC conduit with grey cover, Full plastic, metal reinfored, IP 67",25,18.998681298546053,{"$f":"F3204*(1-Elteq!$F$6)","v":18.998681298546053}]
["ANAMET-S",6203481,"MPC","MPC conduit with grey cover, Full plastic, metal reinfored, IP 67",10,20.903194582752384,{"$f":"F3205*(1-Elteq!$F$6)","v":20.903194582752384}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},6204090,"MPU","MPU conduit with blue cover, Full plastic, metal reinfored, IP 67",50,7.00489276239791,{"$f":"F3206*(1-Elteq!$F$6)","v":7.00489276239791}]
["ANAMET-S",6204091,"MPU","MPU conduit with blue cover, Full plastic, metal reinfored, IP 67",10,7.7295368412666594,{"$f":"F3207*(1-Elteq!$F$6)","v":7.7295368412666594}]
["ANAMET-S",6204110,"MPU","MPU conduit with blue cover, Full plastic, metal reinfored, IP 67",50,7.9896654849631341,{"$f":"F3208*(1-Elteq!$F$6)","v":7.9896654849631341}]
["ANAMET-S",6204111,"MPU","MPU conduit with blue cover, Full plastic, metal reinfored, IP 67",10,8.8072126508663384,{"$f":"F3209*(1-Elteq!$F$6)","v":8.8072126508663384}]
["ANAMET-S",6204130,"MPU","MPU conduit with blue cover, Full plastic, metal reinfored, IP 67",50,9.0673412945628122,{"$f":"F3210*(1-Elteq!$F$6)","v":9.0673412945628122}]
["ANAMET-S",6204131,"MPU","MPU conduit with blue cover, Full plastic, metal reinfored, IP 67",10,9.9777915475004715,{"$f":"F3211*(1-Elteq!$F$6)","v":9.9777915475004715}]
["ANAMET-S",6204160,"MPU","MPU conduit with blue cover, Full plastic, metal reinfored, IP 67",50,9.8941787691694625,{"$f":"F3212*(1-Elteq!$F$6)","v":9.8941787691694625}]
["ANAMET-S",6204161,"MPU","MPU conduit with blue cover, Full plastic, metal reinfored, IP 67",10,10.888241800438133,{"$f":"F3213*(1-Elteq!$F$6)","v":10.888241800438133}]
["ANAMET-S",6204210,"MPU","MPU conduit with blue cover, Full plastic, metal reinfored, IP 67",50,10.76746778729334,{"$f":"F3214*(1-Elteq!$F$6)","v":10.76746778729334}]
["ANAMET-S",6204211,"MPU","MPU conduit with blue cover, Full plastic, metal reinfored, IP 67",10,11.845143596893019,{"$f":"F3215*(1-Elteq!$F$6)","v":11.845143596893019}]
["ANAMET-S",6204290,"MPU","MPU conduit with blue cover, Full plastic, metal reinfored, IP 67",25,16.062943748257275,{"$f":"F3216*(1-Elteq!$F$6)","v":16.062943748257275}]
["ANAMET-S",6204291,"MPU","MPU conduit with blue cover, Full plastic, metal reinfored, IP 67",10,17.679457462656792,{"$f":"F3217*(1-Elteq!$F$6)","v":17.679457462656792}]
["ANAMET-S",6204360,"MPU","MPU conduit with blue cover, Full plastic, metal reinfored, IP 67",25,23.086417128062081,{"$f":"F3218*(1-Elteq!$F$6)","v":23.086417128062081}]
["ANAMET-S",6204361,"MPU","MPU conduit with blue cover, Full plastic, metal reinfored, IP 67",10,25.399703995220008,{"$f":"F3219*(1-Elteq!$F$6)","v":25.399703995220008}]
["ANAMET-S",6204420,"MPU","MPU conduit with blue cover, Full plastic, metal reinfored, IP 67",25,29.961245568611748,{"$f":"F3220*(1-Elteq!$F$6)","v":29.961245568611748}]
["ANAMET-S",6204421,"MPU","MPU conduit with blue cover, Full plastic, metal reinfored, IP 67",10,32.962015279824641,{"$f":"F3221*(1-Elteq!$F$6)","v":32.962015279824641}]
["ANAMET-S",6204480,"MPU","MPU conduit with blue cover, Full plastic, metal reinfored, IP 67",25,34.346271276638028,{"$f":"F3222*(1-Elteq!$F$6)","v":34.346271276638028}]
["ANAMET-S",6204481,"MPU","MPU conduit with blue cover, Full plastic, metal reinfored, IP 67",10,37.774395188209411,{"$f":"F3223*(1-Elteq!$F$6)","v":37.774395188209411}]
["ANAMET-S",6505092,"ADU-K","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",50,2.5641252021509588,{"$f":"F3224*(1-Elteq!$F$6)","v":2.5641252021509588}]
["ANAMET-S",6505112,"ADU-K","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",50,3.2887692810197087,{"$f":"F3225*(1-Elteq!$F$6)","v":3.2887692810197087}]
["ANAMET-S",6505132,"ADU-K","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",50,4.0134133598884576,{"$f":"F3226*(1-Elteq!$F$6)","v":4.0134133598884576}]
["ANAMET-S",6505162,"ADU-K","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",50,5.1096697868950267,{"$f":"F3227*(1-Elteq!$F$6)","v":5.1096697868950267}]
["ANAMET-S",6505212,"ADU-K","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",25,6.0108297311292409,{"$f":"F3228*(1-Elteq!$F$6)","v":6.0108297311292409}]
["ANAMET-S",6505292,"ADU-K","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",25,10.76746778729334,{"$f":"F3229*(1-Elteq!$F$6)","v":10.76746778729334}]
["ANAMET-S",6505362,"ADU-K","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",25,15.700621708822899,{"$f":"F3230*(1-Elteq!$F$6)","v":15.700621708822899}]
["ANAMET-S",6505422,"ADU-K","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",25,16.750426592312245,{"$f":"F3231*(1-Elteq!$F$6)","v":16.750426592312245}]
["ANAMET-S",6505482,"ADU-K","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",10,18.627068950408237,{"$f":"F3232*(1-Elteq!$F$6)","v":18.627068950408237}]
["ANAMET-S",6506093,"ADU-H","Sealtite fittings for MPC/MPU, Straight swivel box connector, IP 54",50,5.1096697868950267,{"$f":"F3233*(1-Elteq!$F$6)","v":5.1096697868950267}]
["ANAMET-S",6506113,"ADU-H","Sealtite fittings for MPC/MPU, Straight swivel box connector, IP 54",50,5.2861856522604924,{"$f":"F3234*(1-Elteq!$F$6)","v":5.2861856522604924}]
["ANAMET-S",6506133,"ADU-H","Sealtite fittings for MPC/MPU, Straight swivel box connector, IP 54",50,5.4719918263294023,{"$f":"F3235*(1-Elteq!$F$6)","v":5.4719918263294023}]
["ANAMET-S",6506163,"ADU-H","Sealtite fittings for MPC/MPU, Straight swivel box connector, IP 54",50,5.6577980003983122,{"$f":"F3236*(1-Elteq!$F$6)","v":5.6577980003983122}]
["ANAMET-S",6506213,"ADU-H","Sealtite fittings for MPC/MPU, Straight swivel box connector, IP 54",25,6.2059262139015967,{"$f":"F3237*(1-Elteq!$F$6)","v":6.2059262139015967}]
["ANAMET-S",6506293,"ADU-H","Sealtite fittings for MPC/MPU, Straight swivel box connector, IP 54",25,6.7633447361083272,{"$f":"F3238*(1-Elteq!$F$6)","v":6.7633447361083272}]
["ANAMET-S",6507092,"AUK-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",50,7.1906989364668199,{"$f":"F3239*(1-Elteq!$F$6)","v":7.1906989364668199}]
["ANAMET-S",6507112,"AUK-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",50,7.1906989364668199,{"$f":"F3240*(1-Elteq!$F$6)","v":7.1906989364668199}]
["ANAMET-S",6507132,"AUK-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",50,7.5344403584943027,{"$f":"F3241*(1-Elteq!$F$6)","v":7.5344403584943027}]
["ANAMET-S",6507162,"AUK-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",50,10.349403895638291,{"$f":"F3242*(1-Elteq!$F$6)","v":10.349403895638291}]
["ANAMET-S",6507212,"AUK-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",25,12.291078414658402,{"$f":"F3243*(1-Elteq!$F$6)","v":12.291078414658402}]
["ANAMET-S",6507292,"AUK-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",25,16.629652579167452,{"$f":"F3244*(1-Elteq!$F$6)","v":16.629652579167452}]
["ANAMET-S",6507362,"AUK-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",25,27.127701414060873,{"$f":"F3245*(1-Elteq!$F$6)","v":27.127701414060873}]
["ANAMET-S",6507422,"AUK-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",10,46.5908981477792,{"$f":"F3246*(1-Elteq!$F$6)","v":46.5908981477792}]
["ANAMET-S",6507482,"AUK-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",10,46.5908981477792,{"$f":"F3247*(1-Elteq!$F$6)","v":46.5908981477792}]
["ANAMET-S",6508094,"AUM-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",50,7.8131496195976684,{"$f":"F3248*(1-Elteq!$F$6)","v":7.8131496195976684}]
["ANAMET-S",6508114,"AUM-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",50,10.442306982672747,{"$f":"F3249*(1-Elteq!$F$6)","v":10.442306982672747}]
["ANAMET-S",6508134,"AUM-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",50,10.442306982672747,{"$f":"F3250*(1-Elteq!$F$6)","v":10.442306982672747}]
["ANAMET-S",6508164,"AUM-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",50,11.547853718382761,{"$f":"F3251*(1-Elteq!$F$6)","v":11.547853718382761}]
["ANAMET-S",6508214,"AUM-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",25,16.546039800836443,{"$f":"F3252*(1-Elteq!$F$6)","v":16.546039800836443}]
["ANAMET-S",6508294,"AUM-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",25,25.2138978211511,{"$f":"F3253*(1-Elteq!$F$6)","v":25.2138978211511}]
["ANAMET-S",6508364,"AUM-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",25,42.410259231228729,{"$f":"F3254*(1-Elteq!$F$6)","v":42.410259231228729}]
["ANAMET-S",6508424,"AUM-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",10,68.265188352917576,{"$f":"F3255*(1-Elteq!$F$6)","v":68.265188352917576}]
["ANAMET-S",6508484,"AUM-P","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",10,69.593702497510264,{"$f":"F3256*(1-Elteq!$F$6)","v":69.593702497510264}]
["ANAMET-S",6513162,"ADU-KM","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",50,2.5641252021509588,{"$f":"F3257*(1-Elteq!$F$6)","v":2.5641252021509588}]
["ANAMET-S",6513202,"ADU-KM","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",50,3.2887692810197087,{"$f":"F3258*(1-Elteq!$F$6)","v":3.2887692810197087}]
["ANAMET-S",6513252,"ADU-KM","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",50,5.1096697868950267,{"$f":"F3259*(1-Elteq!$F$6)","v":5.1096697868950267}]
["ANAMET-S",6513322,"ADU-KM","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",25,6.0108297311292409,{"$f":"F3260*(1-Elteq!$F$6)","v":6.0108297311292409}]
["ANAMET-S",6513402,"ADU-KM","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",25,10.76746778729334,{"$f":"F3261*(1-Elteq!$F$6)","v":10.76746778729334}]
["ANAMET-S",6513502,"ADU-KM","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",25,15.700621708822899,{"$f":"F3262*(1-Elteq!$F$6)","v":15.700621708822899}]
["ANAMET-S",6513632,"ADU-KM","Sealtite fittings for MPC/MPU, Straight swivel with male thread, IP 54",10,18.627068950408237,{"$f":"F3263*(1-Elteq!$F$6)","v":18.627068950408237}]
["ANAMET-S",6517162,"AUK-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",50,5.9829588050189049,{"$f":"F3264*(1-Elteq!$F$6)","v":5.9829588050189049}]
["ANAMET-S",6517172,"AUK-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",50,6.939860601473792,{"$f":"F3265*(1-Elteq!$F$6)","v":6.939860601473792}]
["ANAMET-S",6517202,"AUK-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",50,10.275081426010727,{"$f":"F3266*(1-Elteq!$F$6)","v":10.275081426010727}]
["ANAMET-S",6517252,"AUK-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",50,12.012369153555037,{"$f":"F3267*(1-Elteq!$F$6)","v":12.012369153555037}]
["ANAMET-S",6517322,"AUK-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",25,16.462427022505434,{"$f":"F3268*(1-Elteq!$F$6)","v":16.462427022505434}]
["ANAMET-S",6517402,"AUK-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",25,25.984993443537075,{"$f":"F3269*(1-Elteq!$F$6)","v":25.984993443537075}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},6517502,"AUK-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",25,44.816449185421114,{"$f":"F3270*(1-Elteq!$F$6)","v":44.816449185421114}]
["ANAMET-S",6517632,"AUK-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",10,46.5908981477792,{"$f":"F3271*(1-Elteq!$F$6)","v":46.5908981477792}]
["ANAMET-S",6518124,"AUP-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",50,8.20334258514238,{"$f":"F3272*(1-Elteq!$F$6)","v":8.20334258514238}]
["ANAMET-S",6518164,"AUP-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",50,10.962564270065695,{"$f":"F3273*(1-Elteq!$F$6)","v":10.962564270065695}]
["ANAMET-S",6518174,"AUP-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",50,10.962564270065695,{"$f":"F3274*(1-Elteq!$F$6)","v":10.962564270065695}]
["ANAMET-S",6518204,"AUP-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",50,12.123852857996384,{"$f":"F3275*(1-Elteq!$F$6)","v":12.123852857996384}]
["ANAMET-S",6518254,"AUP-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",25,15.579847695678112,{"$f":"F3276*(1-Elteq!$F$6)","v":15.579847695678112}]
["ANAMET-S",6518324,"AUP-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",25,26.477379804819687,{"$f":"F3277*(1-Elteq!$F$6)","v":26.477379804819687}]
["ANAMET-S",6518404,"AUP-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",25,44.528449615614299,{"$f":"F3278*(1-Elteq!$F$6)","v":44.528449615614299}]
["ANAMET-S",6518504,"AUP-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",10,71.674731647082069,{"$f":"F3279*(1-Elteq!$F$6)","v":71.674731647082069}]
["ANAMET-S",6518634,"AUP-M","Sealtite fittings for MPC/MPU, Straight fixed with male thread, IP 67",10,73.077568261302332,{"$f":"F3280*(1-Elteq!$F$6)","v":73.077568261302332}]
["ANAMET-S",8011070," WL-PA 6L - B  7,5","PA6L polyamide conduit black, Corrugated nylon conduit, IP 67",50,0.8454180920135409,{"$f":"F3281*(1-Elteq!$F$6)","v":0.8454180920135409}]
["ANAMET-S",8011075," WL-PA 6L - B  7,5","PA6L polyamide conduit black, Corrugated nylon conduit, IP 67",5000,0.8454180920135409,{"$f":"F3282*(1-Elteq!$F$6)","v":0.8454180920135409}]
["ANAMET-S",8011100," WL-PA 6L - B 10","PA6L polyamide conduit black, Corrugated nylon conduit, IP 67",50,0.85470840071698639,{"$f":"F3283*(1-Elteq!$F$6)","v":0.85470840071698639}]
["ANAMET-S",8011105," WL-PA 6L - B 10","PA6L polyamide conduit black, Corrugated nylon conduit, IP 67",3000,0.85470840071698639,{"$f":"F3284*(1-Elteq!$F$6)","v":0.85470840071698639}]
["ANAMET-S",8011120," WL-PA 6L - B 12","PA6L polyamide conduit black, Corrugated nylon conduit, IP 67",50,1.1334176618203515,{"$f":"F3285*(1-Elteq!$F$6)","v":1.1334176618203515}]
["ANAMET-S",8011125," WL-PA 6L - B 12","PA6L polyamide conduit black, Corrugated nylon conduit, IP 67",2200,1.1334176618203515,{"$f":"F3286*(1-Elteq!$F$6)","v":1.1334176618203515}]
["ANAMET-S",8011170," WL-PA 6L - B 17","PA6L polyamide conduit black, Corrugated nylon conduit, IP 67",50,1.7651586536546457,{"$f":"F3287*(1-Elteq!$F$6)","v":1.7651586536546457}]
["ANAMET-S",8011175," WL-PA 6L - B 17","PA6L polyamide conduit black, Corrugated nylon conduit, IP 67",1100,1.7651586536546457,{"$f":"F3288*(1-Elteq!$F$6)","v":1.7651586536546457}]
["ANAMET-S",8011230," WL-PA 6L - B 23","PA6L polyamide conduit black, Corrugated nylon conduit, IP 67",50,2.7778023023302061,{"$f":"F3289*(1-Elteq!$F$6)","v":2.7778023023302061}]
["ANAMET-S",8011235," WL-PA 6L - B 23","PA6L polyamide conduit black, Corrugated nylon conduit, IP 67",650,2.7778023023302061,{"$f":"F3290*(1-Elteq!$F$6)","v":2.7778023023302061}]
["ANAMET-S",8011290,"WL-PA 6L - B 29","PA6L polyamide conduit black, Corrugated nylon conduit, IP 67",25,3.4467045289782821,{"$f":"F3291*(1-Elteq!$F$6)","v":3.4467045289782821}]
["ANAMET-S",8011295,"WL-PA 6L - B 29","PA6L polyamide conduit black, Corrugated nylon conduit, IP 67",450,3.4467045289782821,{"$f":"F3292*(1-Elteq!$F$6)","v":3.4467045289782821}]
["ANAMET-S",8011360,"WL-PA 6L - B 36","PA6L polyamide conduit black, Corrugated nylon conduit, IP 67",25,4.9238636128261177,{"$f":"F3293*(1-Elteq!$F$6)","v":4.9238636128261177}]
["ANAMET-S",8011365,"WL-PA 6L - B 36","PA6L polyamide conduit black, Corrugated nylon conduit, IP 67",250,4.9238636128261177,{"$f":"F3294*(1-Elteq!$F$6)","v":4.9238636128261177}]
["ANAMET-S",8011480,"WL-PA 6L - B 48","PA6L polyamide conduit black, Corrugated nylon conduit, IP 67",25,6.958441218880683,{"$f":"F3295*(1-Elteq!$F$6)","v":6.958441218880683}]
["ANAMET-S",8011485,"WL-PA 6L - B 48","PA6L polyamide conduit black, Corrugated nylon conduit, IP 67",150,6.958441218880683,{"$f":"F3296*(1-Elteq!$F$6)","v":6.958441218880683}]
["ANAMET-S",8013050,"WL-PA 6S - B  4,5","PA6S polyamide conduit black, Corrugated nylon conduit, IP 67",100,0.95690179645488693,{"$f":"F3297*(1-Elteq!$F$6)","v":0.95690179645488693}]
["ANAMET-S",8013055,"WL-PA 6S - B  4,5","PA6S polyamide conduit black, Corrugated nylon conduit, IP 67",5000,0.95690179645488693,{"$f":"F3298*(1-Elteq!$F$6)","v":0.95690179645488693}]
["ANAMET-S",8013070,"WL-PA 6S - B  7,5","PA6S polyamide conduit black, Corrugated nylon conduit, IP 67",50,0.92903087034455045,{"$f":"F3299*(1-Elteq!$F$6)","v":0.92903087034455045}]
["ANAMET-S",8013075,"WL-PA 6S - B  7,5","PA6S polyamide conduit black, Corrugated nylon conduit, IP 67",5000,0.92903087034455045,{"$f":"F3300*(1-Elteq!$F$6)","v":0.92903087034455045}]
["ANAMET-S",8013100,"WL-PA 6S - B 10","PA6S polyamide conduit black, Corrugated nylon conduit, IP 67",50,0.95690179645488693,{"$f":"F3301*(1-Elteq!$F$6)","v":0.95690179645488693}]
["ANAMET-S",8013105,"WL-PA 6S - B 10","PA6S polyamide conduit black, Corrugated nylon conduit, IP 67",3000,0.95690179645488693,{"$f":"F3302*(1-Elteq!$F$6)","v":0.95690179645488693}]
["ANAMET-S",8013120,"WL-PA 6S - B 12","PA6S polyamide conduit black, Corrugated nylon conduit, IP 67",50,1.5886427882891812,{"$f":"F3303*(1-Elteq!$F$6)","v":1.5886427882891812}]
["ANAMET-S",8013125,"WL-PA 6S - B 12","PA6S polyamide conduit black, Corrugated nylon conduit, IP 67",2200,1.5886427882891812,{"$f":"F3304*(1-Elteq!$F$6)","v":1.5886427882891812}]
["ANAMET-S",8013170,"WL-PA 6S - B 17","PA6S polyamide conduit black, Corrugated nylon conduit, IP 67",50,2.2203837801234756,{"$f":"F3305*(1-Elteq!$F$6)","v":2.2203837801234756}]
["ANAMET-S",8013175,"WL-PA 6S - B 17","PA6S polyamide conduit black, Corrugated nylon conduit, IP 67",1100,2.2203837801234756,{"$f":"F3306*(1-Elteq!$F$6)","v":2.2203837801234756}]
["ANAMET-S",8013230,"WL-PA 6S - B 23","PA6S polyamide conduit black, Corrugated nylon conduit, IP 67",50,3.3259305158334906,{"$f":"F3307*(1-Elteq!$F$6)","v":3.3259305158334906}]
["ANAMET-S",8013235,"WL-PA 6S - B 23","PA6S polyamide conduit black, Corrugated nylon conduit, IP 67",650,3.3259305158334906,{"$f":"F3308*(1-Elteq!$F$6)","v":3.3259305158334906}]
["ANAMET-S",8013290,"WL-PA 6S - B 29","PA6S polyamide conduit black, Corrugated nylon conduit, IP 67",25,4.4779287950607332,{"$f":"F3309*(1-Elteq!$F$6)","v":4.4779287950607332}]
["ANAMET-S",8013295,"WL-PA 6S - B 29","PA6S polyamide conduit black, Corrugated nylon conduit, IP 67",450,4.4779287950607332,{"$f":"F3310*(1-Elteq!$F$6)","v":4.4779287950607332}]
["ANAMET-S",8013360,"WL-PA 6S - B 36","PA6S polyamide conduit black, Corrugated nylon conduit, IP 67",25,6.1873455964947057,{"$f":"F3311*(1-Elteq!$F$6)","v":6.1873455964947057}]
["ANAMET-S",8013365,"WL-PA 6S - B 36","PA6S polyamide conduit black, Corrugated nylon conduit, IP 67",250,6.1873455964947057,{"$f":"F3312*(1-Elteq!$F$6)","v":6.1873455964947057}]
["ANAMET-S",8013480,"WL-PA 6S - B 48","PA6S polyamide conduit black, Corrugated nylon conduit, IP 67",25,7.8317302370045585,{"$f":"F3313*(1-Elteq!$F$6)","v":7.8317302370045585}]
["ANAMET-S",8013485,"WL-PA 6S - B 48","PA6S polyamide conduit black, Corrugated nylon conduit, IP 67",150,7.8317302370045585,{"$f":"F3314*(1-Elteq!$F$6)","v":7.8317302370045585}]
["ANAMET-S",8012070,"WL-PA 6S - G 7,5","PA6S polyamide conduit grey, Corrugated nylon conduit, IP 67",50,0.92903087034455045,{"$f":"F3315*(1-Elteq!$F$6)","v":0.92903087034455045}]
["ANAMET-S",8012075,"WL-PA 6S - G 7,5","PA6S polyamide conduit grey, Corrugated nylon conduit, IP 67",5000,0.92903087034455045,{"$f":"F3316*(1-Elteq!$F$6)","v":0.92903087034455045}]
["ANAMET-S",8012100,"WL-PA 6S - G 10","PA6S polyamide conduit grey, Corrugated nylon conduit, IP 67",50,0.95690179645488693,{"$f":"F3317*(1-Elteq!$F$6)","v":0.95690179645488693}]
["ANAMET-S",8012105,"WL-PA 6S - G 10","PA6S polyamide conduit grey, Corrugated nylon conduit, IP 67",3000,0.95690179645488693,{"$f":"F3318*(1-Elteq!$F$6)","v":0.95690179645488693}]
["ANAMET-S",8012120,"WL-PA 6S - G 12","PA6S polyamide conduit grey, Corrugated nylon conduit, IP 67",50,1.5886427882891812,{"$f":"F3319*(1-Elteq!$F$6)","v":1.5886427882891812}]
["ANAMET-S",8012125,"WL-PA 6S - G 12","PA6S polyamide conduit grey, Corrugated nylon conduit, IP 67",2200,1.5886427882891812,{"$f":"F3320*(1-Elteq!$F$6)","v":1.5886427882891812}]
["ANAMET-S",8012170,"WL-PA 6S - G 17","PA6S polyamide conduit grey, Corrugated nylon conduit, IP 67",50,2.2203837801234756,{"$f":"F3321*(1-Elteq!$F$6)","v":2.2203837801234756}]
["ANAMET-S",8012175,"WL-PA 6S - G 17","PA6S polyamide conduit grey, Corrugated nylon conduit, IP 67",1100,2.2203837801234756,{"$f":"F3322*(1-Elteq!$F$6)","v":2.2203837801234756}]
["ANAMET-S",8012230,"WL-PA 6S - G 23","PA6S polyamide conduit grey, Corrugated nylon conduit, IP 67",50,3.3259305158334906,{"$f":"F3323*(1-Elteq!$F$6)","v":3.3259305158334906}]
["ANAMET-S",8012235,"WL-PA 6S - G 23","PA6S polyamide conduit grey, Corrugated nylon conduit, IP 67",650,3.3259305158334906,{"$f":"F3324*(1-Elteq!$F$6)","v":3.3259305158334906}]
["ANAMET-S",8012290,"WL-PA 6S - G 29","PA6S polyamide conduit grey, Corrugated nylon conduit, IP 67",25,4.4779287950607332,{"$f":"F3325*(1-Elteq!$F$6)","v":4.4779287950607332}]
["ANAMET-S",8012295,"WL-PA 6S - G 29","PA6S polyamide conduit grey, Corrugated nylon conduit, IP 67",450,4.4779287950607332,{"$f":"F3326*(1-Elteq!$F$6)","v":4.4779287950607332}]
["ANAMET-S",8012360,"WL-PA 6S - G 36","PA6S polyamide conduit grey, Corrugated nylon conduit, IP 67",25,6.1873455964947057,{"$f":"F3327*(1-Elteq!$F$6)","v":6.1873455964947057}]
["ANAMET-S",8012365,"WL-PA 6S - G 36","PA6S polyamide conduit grey, Corrugated nylon conduit, IP 67",250,6.1873455964947057,{"$f":"F3328*(1-Elteq!$F$6)","v":6.1873455964947057}]
["ANAMET-S",8012480,"WL-PA 6S - G 48","PA6S polyamide conduit grey, Corrugated nylon conduit, IP 67",25,7.8317302370045585,{"$f":"F3329*(1-Elteq!$F$6)","v":7.8317302370045585}]
["ANAMET-S",8012485,"WL-PA 6S - G 48","PA6S polyamide conduit grey, Corrugated nylon conduit, IP 67",150,7.8317302370045585,{"$f":"F3330*(1-Elteq!$F$6)","v":7.8317302370045585}]
["ANAMET-S",8015070,"UFW-PA 6HB - B  7,5","PA6UFW polyamide conduit black, Corrugated nylon conduit, IP 67",50,0.92903087034455045,{"$f":"F3331*(1-Elteq!$F$6)","v":0.92903087034455045}]
["ANAMET-S",8015075,"UFW-PA 6HB - B  7,5","PA6UFW polyamide conduit black, Corrugated nylon conduit, IP 67",5000,0.92903087034455045,{"$f":"F3332*(1-Elteq!$F$6)","v":0.92903087034455045}]
["ANAMET-S",8015100,"UFW-PA 6HB - B  10","PA6UFW polyamide conduit black, Corrugated nylon conduit, IP 67",50,0.95690179645488693,{"$f":"F3333*(1-Elteq!$F$6)","v":0.95690179645488693}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8015105,"UFW-PA 6HB - B  10","PA6UFW polyamide conduit black, Corrugated nylon conduit, IP 67",3000,0.95690179645488693,{"$f":"F3334*(1-Elteq!$F$6)","v":0.95690179645488693}]
["ANAMET-S",8015120,"UFW-PA 6HB - B  12","PA6UFW polyamide conduit black, Corrugated nylon conduit, IP 67",50,1.5886427882891812,{"$f":"F3335*(1-Elteq!$F$6)","v":1.5886427882891812}]
["ANAMET-S",8015125,"UFW-PA 6HB - B  12","PA6UFW polyamide conduit black, Corrugated nylon conduit, IP 67",2200,1.5886427882891812,{"$f":"F3336*(1-Elteq!$F$6)","v":1.5886427882891812}]
["ANAMET-S",8015170,"UFW-PA 6HB - B  17","PA6UFW polyamide conduit black, Corrugated nylon conduit, IP 67",50,2.2203837801234756,{"$f":"F3337*(1-Elteq!$F$6)","v":2.2203837801234756}]
["ANAMET-S",8015175,"UFW-PA 6HB - B  17","PA6UFW polyamide conduit black, Corrugated nylon conduit, IP 67",1100,2.2203837801234756,{"$f":"F3338*(1-Elteq!$F$6)","v":2.2203837801234756}]
["ANAMET-S",8015230,"UFW-PA 6HB - B  23","PA6UFW polyamide conduit black, Corrugated nylon conduit, IP 67",50,3.3259305158334906,{"$f":"F3339*(1-Elteq!$F$6)","v":3.3259305158334906}]
["ANAMET-S",8015235,"UFW-PA 6HB - B  23","PA6UFW polyamide conduit black, Corrugated nylon conduit, IP 67",650,3.3259305158334906,{"$f":"F3340*(1-Elteq!$F$6)","v":3.3259305158334906}]
["ANAMET-S",8015290,"UFW-PA 6HB - B  29","PA6UFW polyamide conduit black, Corrugated nylon conduit, IP 67",25,4.4779287950607332,{"$f":"F3341*(1-Elteq!$F$6)","v":4.4779287950607332}]
["ANAMET-S",8015295,"UFW-PA 6HB - B  29","PA6UFW polyamide conduit black, Corrugated nylon conduit, IP 67",450,4.4779287950607332,{"$f":"F3342*(1-Elteq!$F$6)","v":4.4779287950607332}]
["ANAMET-S",8015360,"UFW-PA 6HB - B  36","PA6UFW polyamide conduit black, Corrugated nylon conduit, IP 67",25,6.1873455964947057,{"$f":"F3343*(1-Elteq!$F$6)","v":6.1873455964947057}]
["ANAMET-S",8015365,"UFW-PA 6HB - B  36","PA6UFW polyamide conduit black, Corrugated nylon conduit, IP 67",250,6.1873455964947057,{"$f":"F3344*(1-Elteq!$F$6)","v":6.1873455964947057}]
["ANAMET-S",8017070,"WL-PA 6GV0 - B  7,5","PA6V0 polyamide conduit black, Corrugated nylon conduit, IP 67",50,2.0810291495717932,{"$f":"F3345*(1-Elteq!$F$6)","v":2.0810291495717932}]
["ANAMET-S",8017100,"WL-PA 6GV0 - B 10","PA6V0 polyamide conduit black, Corrugated nylon conduit, IP 67",50,2.1646419279028026,{"$f":"F3346*(1-Elteq!$F$6)","v":2.1646419279028026}]
["ANAMET-S",8017120,"WL-PA 6GV0 - B 12","PA6V0 polyamide conduit black, Corrugated nylon conduit, IP 67",50,3.0936727982473529,{"$f":"F3347*(1-Elteq!$F$6)","v":3.0936727982473529}]
["ANAMET-S",8017170,"WL-PA 6GV0 - B 17","PA6V0 polyamide conduit black, Corrugated nylon conduit, IP 67",50,4.5522512646882971,{"$f":"F3348*(1-Elteq!$F$6)","v":4.5522512646882971}]
["ANAMET-S",8017230,"WL-PA 6GV0 - B 23","PA6V0 polyamide conduit black, Corrugated nylon conduit, IP 67",50,7.5251500497908586,{"$f":"F3349*(1-Elteq!$F$6)","v":7.5251500497908586}]
["ANAMET-S",8017290,"WL-PA 6GV0 - B 29","PA6V0 polyamide conduit black, Corrugated nylon conduit, IP 67",25,9.364631173073068,{"$f":"F3350*(1-Elteq!$F$6)","v":9.364631173073068}]
["ANAMET-S",8017360,"WL-PA 6GV0 - B 36","PA6V0 polyamide conduit black, Corrugated nylon conduit, IP 67",25,13.303722063333963,{"$f":"F3351*(1-Elteq!$F$6)","v":13.303722063333963}]
["ANAMET-S",8017480,"WL-PA 6GV0 - B 48","PA6V0 polyamide conduit black, Corrugated nylon conduit, IP 67",25,18.543456172077228,{"$f":"F3352*(1-Elteq!$F$6)","v":18.543456172077228}]
["ANAMET-S",8025100,"WL-PA 12S - B 10","PA12S polyamide conduit black, Corrugated nylon conduit, IP 67",50,3.0100600199163439,{"$f":"F3353*(1-Elteq!$F$6)","v":3.0100600199163439}]
["ANAMET-S",8025120,"WL-PA 12S - B 12","PA12S polyamide conduit black, Corrugated nylon conduit, IP 67",50,4.0598649034056855,{"$f":"F3354*(1-Elteq!$F$6)","v":4.0598649034056855}]
["ANAMET-S",8025170,"WL-PA 12S - B 17","PA12S polyamide conduit black, Corrugated nylon conduit, IP 67",50,6.2152165226050426,{"$f":"F3355*(1-Elteq!$F$6)","v":6.2152165226050426}]
["ANAMET-S",8025230,"WL-PA 12S - B 23","PA12S polyamide conduit black, Corrugated nylon conduit, IP 67",50,10.293662043417617,{"$f":"F3356*(1-Elteq!$F$6)","v":10.293662043417617}]
["ANAMET-S",8025290,"WL-PA 12S - B 29","PA12S polyamide conduit black, Corrugated nylon conduit, IP 67",25,13.823979350726912,{"$f":"F3357*(1-Elteq!$F$6)","v":13.823979350726912}]
["ANAMET-S",8025360,"WL-PA 12S - B 36","PA12S polyamide conduit black, Corrugated nylon conduit, IP 67",25,21.005387978490283,{"$f":"F3358*(1-Elteq!$F$6)","v":21.005387978490283}]
["ANAMET-S",8025480,"WL-PA 12S - B 48","PA12S polyamide conduit black, Corrugated nylon conduit, IP 67",25,25.288220290778661,{"$f":"F3359*(1-Elteq!$F$6)","v":25.288220290778661}]
["ANAMET-S",8028050,"WL-PP  - B  5","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",100,0.58528944831706675,{"$f":"F3360*(1-Elteq!$F$6)","v":0.58528944831706675}]
["ANAMET-S",8028055,"WL-PP  - B  5","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",9000,0.58528944831706675,{"$f":"F3361*(1-Elteq!$F$6)","v":0.58528944831706675}]
["ANAMET-S",8028060,"WL-PP  - B  6","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",100,0.58528944831706675,{"$f":"F3362*(1-Elteq!$F$6)","v":0.58528944831706675}]
["ANAMET-S",8028065,"WL-PP  - B  6","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",5000,0.58528944831706675,{"$f":"F3363*(1-Elteq!$F$6)","v":0.58528944831706675}]
["ANAMET-S",8028070,"WL-PP  - B  7,5","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",50,0.58528944831706675,{"$f":"F3364*(1-Elteq!$F$6)","v":0.58528944831706675}]
["ANAMET-S",8028075,"WL-PP  - B  7,5","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",5000,0.58528944831706675,{"$f":"F3365*(1-Elteq!$F$6)","v":0.58528944831706675}]
["ANAMET-S",8028100,"WL-PP  - B  10","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",50,0.61316037442740334,{"$f":"F3366*(1-Elteq!$F$6)","v":0.61316037442740334}]
["ANAMET-S",8028105,"WL-PP  - B  10","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",3000,0.61316037442740334,{"$f":"F3367*(1-Elteq!$F$6)","v":0.61316037442740334}]
["ANAMET-S",8028120,"WL-PP  - B  12","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",50,0.80825685719975882,{"$f":"F3368*(1-Elteq!$F$6)","v":0.80825685719975882}]
["ANAMET-S",8028125,"WL-PP  - B  12","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",2000,0.80825685719975882,{"$f":"F3369*(1-Elteq!$F$6)","v":0.80825685719975882}]
["ANAMET-S",8028140,"WL-PP  - B  14","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",50,1.0590951921927874,{"$f":"F3370*(1-Elteq!$F$6)","v":1.0590951921927874}]
["ANAMET-S",8028145,"WL-PP  - B  14","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",1700,1.0590951921927874,{"$f":"F3371*(1-Elteq!$F$6)","v":1.0590951921927874}]
["ANAMET-S",8028170,"WL-PP  - B  17","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",50,1.0776758095996783,{"$f":"F3372*(1-Elteq!$F$6)","v":1.0776758095996783}]
["ANAMET-S",8028175,"WL-PP  - B  17","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",1300,1.0776758095996783,{"$f":"F3373*(1-Elteq!$F$6)","v":1.0776758095996783}]
["ANAMET-S",8028190,"WL-PP  - B  19","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",50,1.3563850707030436,{"$f":"F3374*(1-Elteq!$F$6)","v":1.3563850707030436}]
["ANAMET-S",8028195,"WL-PP  - B  19","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",1000,1.3563850707030436,{"$f":"F3375*(1-Elteq!$F$6)","v":1.3563850707030436}]
["ANAMET-S",8028230,"WL-PP  - B  23","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",50,1.7837392710615367,{"$f":"F3376*(1-Elteq!$F$6)","v":1.7837392710615367}]
["ANAMET-S",8028235,"WL-PP  - B  23","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",700,1.7837392710615367,{"$f":"F3377*(1-Elteq!$F$6)","v":1.7837392710615367}]
["ANAMET-S",8028260,"WL-PP  - B  26","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",25,2.2018031627165846,{"$f":"F3378*(1-Elteq!$F$6)","v":2.2018031627165846}]
["ANAMET-S",8028265,"WL-PP  - B  26","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",600,2.2018031627165846,{"$f":"F3379*(1-Elteq!$F$6)","v":2.2018031627165846}]
["ANAMET-S",8028290,"WL-PP  - B  29","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",25,2.2110934714200297,{"$f":"F3380*(1-Elteq!$F$6)","v":2.2110934714200297}]
["ANAMET-S",8028295,"WL-PP  - B  29","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",500,2.2110934714200297,{"$f":"F3381*(1-Elteq!$F$6)","v":2.2110934714200297}]
["ANAMET-S",8028360,"WL-PP  - B  36","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",25,3.5581882334196284,{"$f":"F3382*(1-Elteq!$F$6)","v":3.5581882334196284}]
["ANAMET-S",8028365,"WL-PP  - B  36","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",300,3.5581882334196284,{"$f":"F3383*(1-Elteq!$F$6)","v":3.5581882334196284}]
["ANAMET-S",8028480,"WL-PP  - B  48","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",25,4.8681217606054448,{"$f":"F3384*(1-Elteq!$F$6)","v":4.8681217606054448}]
["ANAMET-S",8028485,"WL-PP  - B  48","PP-MOD polypropelene black, Corrugated nylon conduit, IP 67",200,4.8681217606054448,{"$f":"F3385*(1-Elteq!$F$6)","v":4.8681217606054448}]
["ANAMET-S",8029070,"WLD-PA - B - 7","PA6 splitable duo conduit, Corrugated nylon conduit, IP 54",50,5.1654116391156997,{"$f":"F3386*(1-Elteq!$F$6)","v":5.1654116391156997}]
["ANAMET-S",8029100,"WLD-PA - B - 10","PA6 splitable duo conduit, Corrugated nylon conduit, IP 54",50,5.7042495439155392,{"$f":"F3387*(1-Elteq!$F$6)","v":5.7042495439155392}]
["ANAMET-S",8029130,"WLD-PA - B - 13","PA6 splitable duo conduit, Corrugated nylon conduit, IP 54",50,7.2836020235012748,{"$f":"F3388*(1-Elteq!$F$6)","v":7.2836020235012748}]
["ANAMET-S",8029160,"WLD-PA - B - 16","PA6 splitable duo conduit, Corrugated nylon conduit, IP 54",50,8.8072126508663384,{"$f":"F3389*(1-Elteq!$F$6)","v":8.8072126508663384}]
["ANAMET-S",8029170,"WLD-PA - B - 17","PA6 splitable duo conduit, Corrugated nylon conduit, IP 54",50,10.832499948217459,{"$f":"F3390*(1-Elteq!$F$6)","v":10.832499948217459}]
["ANAMET-S",8029220,"WLD-PA - B - 22","PA6 splitable duo conduit, Corrugated nylon conduit, IP 54",50,11.761530818562008,{"$f":"F3391*(1-Elteq!$F$6)","v":11.761530818562008}]
["ANAMET-S",8029230,"WLD-PA - B - 23","PA6 splitable duo conduit, Corrugated nylon conduit, IP 54",50,12.040240079665375,{"$f":"F3392*(1-Elteq!$F$6)","v":12.040240079665375}]
["ANAMET-S",8029260,"WLD-PA - B - 26","PA6 splitable duo conduit, Corrugated nylon conduit, IP 54",25,12.356110575582521,{"$f":"F3393*(1-Elteq!$F$6)","v":12.356110575582521}]
["ANAMET-S",8029290,"WLD-PA - B - 29","PA6 splitable duo conduit, Corrugated nylon conduit, IP 54",25,14.725139294961124,{"$f":"F3394*(1-Elteq!$F$6)","v":14.725139294961124}]
["ANAMET-S",8029360,"WLD-PA - B - 37","PA6 splitable duo conduit, Corrugated nylon conduit, IP 54",25,17.18707110137418,{"$f":"F3395*(1-Elteq!$F$6)","v":17.18707110137418}]
["ANAMET-S",8029480,"WLD-PA - B - 50","PA6 splitable duo conduit, Corrugated nylon conduit, IP 54",25,25.028091647082189,{"$f":"F3396*(1-Elteq!$F$6)","v":25.028091647082189}]
["ANAMET-S",8022070,"WLD-PP - B - 7","PP splitable duo conduit, Corrugated nylon conduit, IP 54",50,3.8368974945229932,{"$f":"F3397*(1-Elteq!$F$6)","v":3.8368974945229932}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},8022100,"WLD-PP - B - 10","PP splitable duo conduit, Corrugated nylon conduit, IP 54",50,4.4314772515435052,{"$f":"F3398*(1-Elteq!$F$6)","v":4.4314772515435052}]
["ANAMET-S",8022130,"WLD-PP - B - 13","PP splitable duo conduit, Corrugated nylon conduit, IP 54",50,5.4069596654052834,{"$f":"F3399*(1-Elteq!$F$6)","v":5.4069596654052834}]
["ANAMET-S",8022160,"WLD-PP - B - 16","PP splitable duo conduit, Corrugated nylon conduit, IP 54",50,5.6577980003983122,{"$f":"F3400*(1-Elteq!$F$6)","v":5.6577980003983122}]
["ANAMET-S",8022170,"WLD-PP - B - 17","PP splitable duo conduit, Corrugated nylon conduit, IP 54",50,5.9086363353913409,{"$f":"F3401*(1-Elteq!$F$6)","v":5.9086363353913409}]
["ANAMET-S",8022220,"WLD-PP - B - 22","PP splitable duo conduit, Corrugated nylon conduit, IP 54",50,7.2836020235012748,{"$f":"F3402*(1-Elteq!$F$6)","v":7.2836020235012748}]
["ANAMET-S",8022230,"WLD-PP - B - 23","PP splitable duo conduit, Corrugated nylon conduit, IP 54",50,8.2683747460664989,{"$f":"F3403*(1-Elteq!$F$6)","v":8.2683747460664989}]
["ANAMET-S",8022260,"WLD-PP - B - 26","PP splitable duo conduit, Corrugated nylon conduit, IP 54",25,8.7607611073491096,{"$f":"F3404*(1-Elteq!$F$6)","v":8.7607611073491096}]
["ANAMET-S",8022290,"WLD-PP - B - 29","PP splitable duo conduit, Corrugated nylon conduit, IP 54",25,9.9963721649073616,{"$f":"F3405*(1-Elteq!$F$6)","v":9.9963721649073616}]
["ANAMET-S",8022360,"WLD-PP - B - 37","PP splitable duo conduit, Corrugated nylon conduit, IP 54",25,12.950690332603031,{"$f":"F3406*(1-Elteq!$F$6)","v":12.950690332603031}]
["ANAMET-S",8022480,"WLD-PP - B - 50","PP splitable duo conduit, Corrugated nylon conduit, IP 54",25,16.05365343955383,{"$f":"F3407*(1-Elteq!$F$6)","v":16.05365343955383}]
["ANAMET-S",8023070,"WLD-PPU - B - 7","PP-UV splitable duo conduit, Corrugated nylon conduit, IP 54",50,4.4314772515435052,{"$f":"F3408*(1-Elteq!$F$6)","v":4.4314772515435052}]
["ANAMET-S",8023100,"WLD-PPU - B - 10","PP-UV splitable duo conduit, Corrugated nylon conduit, IP 54",50,4.8681217606054448,{"$f":"F3409*(1-Elteq!$F$6)","v":4.8681217606054448}]
["ANAMET-S",8023130,"WLD-PPU - B - 13","PP-UV splitable duo conduit, Corrugated nylon conduit, IP 54",50,6.1966359051981517,{"$f":"F3410*(1-Elteq!$F$6)","v":6.1966359051981517}]
["ANAMET-S",8023160,"WLD-PPU - B - 16","PP-UV splitable duo conduit, Corrugated nylon conduit, IP 54",50,7.5251500497908586,{"$f":"F3411*(1-Elteq!$F$6)","v":7.5251500497908586}]
["ANAMET-S",8023170,"WLD-PPU - B - 17","PP-UV splitable duo conduit, Corrugated nylon conduit, IP 54",50,9.2066959251144951,{"$f":"F3412*(1-Elteq!$F$6)","v":9.2066959251144951}]
["ANAMET-S",8023220,"WLD-PPU - B - 22","PP-UV splitable duo conduit, Corrugated nylon conduit, IP 54",50,9.9963721649073616,{"$f":"F3413*(1-Elteq!$F$6)","v":9.9963721649073616}]
["ANAMET-S",8023230,"WLD-PPU - B - 23","PP-UV splitable duo conduit, Corrugated nylon conduit, IP 54",50,10.293662043417617,{"$f":"F3414*(1-Elteq!$F$6)","v":10.293662043417617}]
["ANAMET-S",8023260,"WLD-PPU - B - 26","PP-UV splitable duo conduit, Corrugated nylon conduit, IP 54",25,10.544500378410646,{"$f":"F3415*(1-Elteq!$F$6)","v":10.544500378410646}]
["ANAMET-S",8023290,"WLD-PPU - B - 29","PP-UV splitable duo conduit, Corrugated nylon conduit, IP 54",25,12.560497367058321,{"$f":"F3416*(1-Elteq!$F$6)","v":12.560497367058321}]
["ANAMET-S",8023360,"WLD-PPU - B - 37","PP-UV splitable duo conduit, Corrugated nylon conduit, IP 54",25,14.622945899223224,{"$f":"F3417*(1-Elteq!$F$6)","v":14.622945899223224}]
["ANAMET-S",8023480,"WLD-PPU - B - 50","PP-UV splitable duo conduit, Corrugated nylon conduit, IP 54",25,21.386290635331552,{"$f":"F3418*(1-Elteq!$F$6)","v":21.386290635331552}]
["ANAMET-S",2670160,"SVCHF M16 B-12","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",25,6.1594746703843688,{"$f":"F3419*(1-Elteq!$F$6)","v":6.1594746703843688}]
["ANAMET-S",2670161,"SVCHF M16 B-10","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",25,6.0479909659430229,{"$f":"F3420*(1-Elteq!$F$6)","v":6.0479909659430229}]
["ANAMET-S",2670200,"SVCHF M20 B-17","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",25,7.3393438757219478,{"$f":"F3421*(1-Elteq!$F$6)","v":7.3393438757219478}]
["ANAMET-S",2670201,"SVCHF M20 B-12","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",25,6.9863121449910182,{"$f":"F3422*(1-Elteq!$F$6)","v":6.9863121449910182}]
["ANAMET-S",2670202,"SVCHF M20 B-23","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",25,7.5808919020115315,{"$f":"F3423*(1-Elteq!$F$6)","v":7.5808919020115315}]
["ANAMET-S",2670250,"SVCHF M25 B-23","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",25,12.950690332603031,{"$f":"F3424*(1-Elteq!$F$6)","v":12.950690332603031}]
["ANAMET-S",2670251,"SVCHF M25 B-17","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",25,7.9246333240390143,{"$f":"F3425*(1-Elteq!$F$6)","v":7.9246333240390143}]
["ANAMET-S",2670320,"SVCHF M32 B-29","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",10,13.842559968133802,{"$f":"F3426*(1-Elteq!$F$6)","v":13.842559968133802}]
["ANAMET-S",2680120,"SV M12 G-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.3749656881099346,{"$f":"F3427*(1-Elteq!$F$6)","v":1.3749656881099346}]
["ANAMET-S",2680121,"SV M12 G-7,5","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.3192238358892616,{"$f":"F3428*(1-Elteq!$F$6)","v":1.3192238358892616}]
["ANAMET-S",2680160,"SV M16 G-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.5979330969926269,{"$f":"F3429*(1-Elteq!$F$6)","v":1.5979330969926269}]
["ANAMET-S",2680161,"SV M16 G-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.4957397012547262,{"$f":"F3430*(1-Elteq!$F$6)","v":1.4957397012547262}]
["ANAMET-S",2680200,"SV M20 G-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.5514815534753992,{"$f":"F3431*(1-Elteq!$F$6)","v":1.5514815534753992}]
["ANAMET-S",2680201,"SV M20 G-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.5514815534753992,{"$f":"F3432*(1-Elteq!$F$6)","v":1.5514815534753992}]
["ANAMET-S",2680250,"SV M25 G-23","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",25,3.1494146504680258,{"$f":"F3433*(1-Elteq!$F$6)","v":3.1494146504680258}]
["ANAMET-S",2680251,"SV M25 G-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.8859326667994372,{"$f":"F3434*(1-Elteq!$F$6)","v":1.8859326667994372}]
["ANAMET-S",2680320,"SV M32 G-29","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",20,3.9298005815574486,{"$f":"F3435*(1-Elteq!$F$6)","v":3.9298005815574486}]
["ANAMET-S",2680400,"SV M40 G-37","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",10,5.3605081218880555,{"$f":"F3436*(1-Elteq!$F$6)","v":5.3605081218880555}]
["ANAMET-S",2680500,"SV M50 G-48","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",5,6.4660548575980705,{"$f":"F3437*(1-Elteq!$F$6)","v":6.4660548575980705}]
["ANAMET-S",2680630,"SV M63 G-48","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",5,6.9956024536944641,{"$f":"F3438*(1-Elteq!$F$6)","v":6.9956024536944641}]
["ANAMET-S",2681120,"SV M12 B-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.3749656881099346,{"$f":"F3439*(1-Elteq!$F$6)","v":1.3749656881099346}]
["ANAMET-S",2681121,"SV M12 B-7,5","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.3192238358892616,{"$f":"F3440*(1-Elteq!$F$6)","v":1.3192238358892616}]
["ANAMET-S",2681160,"SV M16 B-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.5979330969926269,{"$f":"F3441*(1-Elteq!$F$6)","v":1.5979330969926269}]
["ANAMET-S",2681161,"SV M16 B-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.4957397012547262,{"$f":"F3442*(1-Elteq!$F$6)","v":1.4957397012547262}]
["ANAMET-S",2681200,"SV M20 B-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.5514815534753992,{"$f":"F3443*(1-Elteq!$F$6)","v":1.5514815534753992}]
["ANAMET-S",2681201,"SV M20 B-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.5514815534753992,{"$f":"F3444*(1-Elteq!$F$6)","v":1.5514815534753992}]
["ANAMET-S",2681250,"SV M25 B-23","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",25,3.1494146504680258,{"$f":"F3445*(1-Elteq!$F$6)","v":3.1494146504680258}]
["ANAMET-S",2681251,"SV M25 B-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.8859326667994372,{"$f":"F3446*(1-Elteq!$F$6)","v":1.8859326667994372}]
["ANAMET-S",2681320,"SV M32 B-29","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",20,3.9298005815574486,{"$f":"F3447*(1-Elteq!$F$6)","v":3.9298005815574486}]
["ANAMET-S",2681400,"SV M40 B-37","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",10,5.3605081218880555,{"$f":"F3448*(1-Elteq!$F$6)","v":5.3605081218880555}]
["ANAMET-S",2681500,"SV M50 B-48","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",5,6.4660548575980705,{"$f":"F3449*(1-Elteq!$F$6)","v":6.4660548575980705}]
["ANAMET-S",2681630,"SV M63 B-48","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",5,6.9956024536944641,{"$f":"F3450*(1-Elteq!$F$6)","v":6.9956024536944641}]
["ANAMET-S",2683160,"SV 90 M16 B-12","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",50,3.0565115634335709,{"$f":"F3451*(1-Elteq!$F$6)","v":3.0565115634335709}]
["ANAMET-S",2683161,"SV 90 M16 B-10","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",50,2.907866624178443,{"$f":"F3452*(1-Elteq!$F$6)","v":2.907866624178443}]
["ANAMET-S",2683200,"SV 90 M20 B-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",25,3.59534946823341,{"$f":"F3453*(1-Elteq!$F$6)","v":3.59534946823341}]
["ANAMET-S",2683201,"SV 90 M20 B-12","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",50,3.2980595897231542,{"$f":"F3454*(1-Elteq!$F$6)","v":3.2980595897231542}]
["ANAMET-S",2683250,"SV 90 M25 B-23","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",20,5.0632182433777997,{"$f":"F3455*(1-Elteq!$F$6)","v":5.0632182433777997}]
["ANAMET-S",2683251,"SV 90 M25 B-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",25,3.7997362597092108,{"$f":"F3456*(1-Elteq!$F$6)","v":3.7997362597092108}]
["ANAMET-S",2683320,"SV 90 M32 B-29","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",10,7.8317302370045585,{"$f":"F3457*(1-Elteq!$F$6)","v":7.8317302370045585}]
["ANAMET-S",2683321,"SV 90 M32 B-23","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",20,6.2059262139015967,{"$f":"F3458*(1-Elteq!$F$6)","v":6.2059262139015967}]
["ANAMET-S",2683400,"SV 90 M40 B-36","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",10,12.662690762796222,{"$f":"F3459*(1-Elteq!$F$6)","v":12.662690762796222}]
["ANAMET-S",2683401,"SV 90 M40 B-29","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",10,8.8165029595697835,{"$f":"F3460*(1-Elteq!$F$6)","v":8.8165029595697835}]
["ANAMET-S",2683500,"SV 90 M50 B-48","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",5,15.078171025692054,{"$f":"F3461*(1-Elteq!$F$6)","v":15.078171025692054}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},2683501,"SV 90 M50 B-36","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",10,13.108625580561606,{"$f":"F3462*(1-Elteq!$F$6)","v":13.108625580561606}]
["ANAMET-S",2683630,"SV 90 M63 B-48","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",5,15.719202326229794,{"$f":"F3463*(1-Elteq!$F$6)","v":15.719202326229794}]
["ANAMET-S",2671090,"SVCHF PG 9 B-10","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",25,6.4103130053773976,{"$f":"F3464*(1-Elteq!$F$6)","v":6.4103130053773976}]
["ANAMET-S",2671110,"SVCHF PG11 B-12","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",25,6.5032160924118525,{"$f":"F3465*(1-Elteq!$F$6)","v":6.5032160924118525}]
["ANAMET-S",2671130,"SVCHF PG 13,5 B-17","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",25,7.6830852977494315,{"$f":"F3466*(1-Elteq!$F$6)","v":7.6830852977494315}]
["ANAMET-S",2671131,"SVCHF PG 13,5 B-12","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",25,7.3393438757219478,{"$f":"F3467*(1-Elteq!$F$6)","v":7.3393438757219478}]
["ANAMET-S",2671160,"SVCHF PG 16 B-17","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",25,7.9246333240390143,{"$f":"F3468*(1-Elteq!$F$6)","v":7.9246333240390143}]
["ANAMET-S",2671210,"SVCHF PG 21 B-23","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",25,13.591721633140773,{"$f":"F3469*(1-Elteq!$F$6)","v":13.591721633140773}]
["ANAMET-S",2671290,"SVCHF PG 29 B-29","Fittings for Anaquick conduit, Straight cablehose male thread, IP 68",10,14.530042812188769,{"$f":"F3470*(1-Elteq!$F$6)","v":14.530042812188769}]
["ANAMET-S",2682160,"SV 90 M16 G-12","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",50,3.0565115634335709,{"$f":"F3471*(1-Elteq!$F$6)","v":3.0565115634335709}]
["ANAMET-S",2682161,"SV 90 M16 G-10","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",50,2.907866624178443,{"$f":"F3472*(1-Elteq!$F$6)","v":2.907866624178443}]
["ANAMET-S",2682200,"SV 90 M20 G-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",25,3.59534946823341,{"$f":"F3473*(1-Elteq!$F$6)","v":3.59534946823341}]
["ANAMET-S",2682201,"SV 90 M20 G-12","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",50,3.2980595897231542,{"$f":"F3474*(1-Elteq!$F$6)","v":3.2980595897231542}]
["ANAMET-S",2682250,"SV 90 M25 G-23","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",20,5.0632182433777997,{"$f":"F3475*(1-Elteq!$F$6)","v":5.0632182433777997}]
["ANAMET-S",2682251,"SV 90 M25 G-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",25,3.7997362597092108,{"$f":"F3476*(1-Elteq!$F$6)","v":3.7997362597092108}]
["ANAMET-S",2682320,"SV 90 M32 G-29","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",10,7.8317302370045585,{"$f":"F3477*(1-Elteq!$F$6)","v":7.8317302370045585}]
["ANAMET-S",2682321,"SV 90 M32 G-23","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",20,6.2059262139015967,{"$f":"F3478*(1-Elteq!$F$6)","v":6.2059262139015967}]
["ANAMET-S",2682400,"SV 90 M40 G-36","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",10,12.662690762796222,{"$f":"F3479*(1-Elteq!$F$6)","v":12.662690762796222}]
["ANAMET-S",2682401,"SV 90 M40 G-29","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",10,8.8165029595697835,{"$f":"F3480*(1-Elteq!$F$6)","v":8.8165029595697835}]
["ANAMET-S",2682500,"SV 90 M50 G-48","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",5,15.078171025692054,{"$f":"F3481*(1-Elteq!$F$6)","v":15.078171025692054}]
["ANAMET-S",2682501,"SV 90 M50 G-36","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",10,13.108625580561606,{"$f":"F3482*(1-Elteq!$F$6)","v":13.108625580561606}]
["ANAMET-S",2682630,"SV 90 M63 G-48","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",5,15.719202326229794,{"$f":"F3483*(1-Elteq!$F$6)","v":15.719202326229794}]
["ANAMET-S",2684070,"SV PG 7 G-7,5","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.3192238358892616,{"$f":"F3484*(1-Elteq!$F$6)","v":1.3192238358892616}]
["ANAMET-S",2684071,"SV PG 7 G-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.3749656881099346,{"$f":"F3485*(1-Elteq!$F$6)","v":1.3749656881099346}]
["ANAMET-S",2684090,"SV PG 9 G-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.3749656881099346,{"$f":"F3486*(1-Elteq!$F$6)","v":1.3749656881099346}]
["ANAMET-S",2684091,"SV PG 9 G-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.5236106273650625,{"$f":"F3487*(1-Elteq!$F$6)","v":1.5236106273650625}]
["ANAMET-S",2684110,"SV PG 11 G-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.5236106273650625,{"$f":"F3488*(1-Elteq!$F$6)","v":1.5236106273650625}]
["ANAMET-S",2684111,"SV PG 11 G-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.6350943318064088,{"$f":"F3489*(1-Elteq!$F$6)","v":1.6350943318064088}]
["ANAMET-S",2684130,"SV PG 13 G-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.7001264927305273,{"$f":"F3490*(1-Elteq!$F$6)","v":1.7001264927305273}]
["ANAMET-S",2684131,"SV PG 13 G-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.7001264927305273,{"$f":"F3491*(1-Elteq!$F$6)","v":1.7001264927305273}]
["ANAMET-S",2684160,"SV PG 16 G-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.7837392710615367,{"$f":"F3492*(1-Elteq!$F$6)","v":1.7837392710615367}]
["ANAMET-S",2684210,"SV PG 21 G-23","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",25,3.7904459510057658,{"$f":"F3493*(1-Elteq!$F$6)","v":3.7904459510057658}]
["ANAMET-S",2684290,"SV PG 29 G-29","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",20,4.1248970643298044,{"$f":"F3494*(1-Elteq!$F$6)","v":4.1248970643298044}]
["ANAMET-S",2684360,"SV PG 36 G-36","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",10,5.3605081218880555,{"$f":"F3495*(1-Elteq!$F$6)","v":5.3605081218880555}]
["ANAMET-S",2684480,"SV PG 48 G-48","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",5,7.0885055407289199,{"$f":"F3496*(1-Elteq!$F$6)","v":7.0885055407289199}]
["ANAMET-S",2685070,"SV PG 7 B-7,5","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.3192238358892616,{"$f":"F3497*(1-Elteq!$F$6)","v":1.3192238358892616}]
["ANAMET-S",2685071,"SV PG 7 B-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.3749656881099346,{"$f":"F3498*(1-Elteq!$F$6)","v":1.3749656881099346}]
["ANAMET-S",2685090,"SV PG 9 B-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.3749656881099346,{"$f":"F3499*(1-Elteq!$F$6)","v":1.3749656881099346}]
["ANAMET-S",2685091,"SV PG 9 B-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.5236106273650625,{"$f":"F3500*(1-Elteq!$F$6)","v":1.5236106273650625}]
["ANAMET-S",2685110,"SV PG 11 B-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.5236106273650625,{"$f":"F3501*(1-Elteq!$F$6)","v":1.5236106273650625}]
["ANAMET-S",2685111,"SV PG 11 B-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.6350943318064088,{"$f":"F3502*(1-Elteq!$F$6)","v":1.6350943318064088}]
["ANAMET-S",2685130,"SV PG 13 B-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.7001264927305273,{"$f":"F3503*(1-Elteq!$F$6)","v":1.7001264927305273}]
["ANAMET-S",2685131,"SV PG 13 B-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.7001264927305273,{"$f":"F3504*(1-Elteq!$F$6)","v":1.7001264927305273}]
["ANAMET-S",2685160,"SV PG 16 B-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",50,1.7837392710615367,{"$f":"F3505*(1-Elteq!$F$6)","v":1.7837392710615367}]
["ANAMET-S",2685210,"SV PG 21 B-23","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",25,3.7904459510057658,{"$f":"F3506*(1-Elteq!$F$6)","v":3.7904459510057658}]
["ANAMET-S",2685290,"SV PG 29 B-29","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",20,4.1248970643298044,{"$f":"F3507*(1-Elteq!$F$6)","v":4.1248970643298044}]
["ANAMET-S",2685360,"SV PG 36 B-36","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",10,5.3605081218880555,{"$f":"F3508*(1-Elteq!$F$6)","v":5.3605081218880555}]
["ANAMET-S",2685480,"SV PG 48 B-48","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",5,7.0885055407289199,{"$f":"F3509*(1-Elteq!$F$6)","v":7.0885055407289199}]
["ANAMET-S",2686090,"SV 90 PG 9 G-10","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",50,2.907866624178443,{"$f":"F3510*(1-Elteq!$F$6)","v":2.907866624178443}]
["ANAMET-S",2686110,"SV 90 PG 11 G-12","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",50,3.2051565026886988,{"$f":"F3511*(1-Elteq!$F$6)","v":3.2051565026886988}]
["ANAMET-S",2686130,"SV 90 PG 13 G-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",25,3.4002529854610546,{"$f":"F3512*(1-Elteq!$F$6)","v":3.4002529854610546}]
["ANAMET-S",2686160,"SV 90 PG 16 G-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",25,3.5488979247161825,{"$f":"F3513*(1-Elteq!$F$6)","v":3.5488979247161825}]
["ANAMET-S",2686210,"SV 90 PG 21 G-23","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",20,5.0632182433777997,{"$f":"F3514*(1-Elteq!$F$6)","v":5.0632182433777997}]
["ANAMET-S",2686290,"SV 90 PG 29 G-29","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",10,7.8317302370045585,{"$f":"F3515*(1-Elteq!$F$6)","v":7.8317302370045585}]
["ANAMET-S",2686360,"SV 90 PG 36 G-36","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",10,12.662690762796222,{"$f":"F3516*(1-Elteq!$F$6)","v":12.662690762796222}]
["ANAMET-S",2686480,"SV 90 PG 48 G-48","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",5,15.672750782712566,{"$f":"F3517*(1-Elteq!$F$6)","v":15.672750782712566}]
["ANAMET-S",2687090,"SV 90 PG 9 B-10","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",50,2.907866624178443,{"$f":"F3518*(1-Elteq!$F$6)","v":2.907866624178443}]
["ANAMET-S",2687110,"SV 90 PG 11 B-12","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",50,3.2051565026886988,{"$f":"F3519*(1-Elteq!$F$6)","v":3.2051565026886988}]
["ANAMET-S",2687130,"SV 90 PG 13 B-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",25,3.4002529854610546,{"$f":"F3520*(1-Elteq!$F$6)","v":3.4002529854610546}]
["ANAMET-S",2687160,"SV 90 PG 16 B-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",25,3.5488979247161825,{"$f":"F3521*(1-Elteq!$F$6)","v":3.5488979247161825}]
["ANAMET-S",2687210,"SV 90 PG 21 B-23","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",20,5.0632182433777997,{"$f":"F3522*(1-Elteq!$F$6)","v":5.0632182433777997}]
["ANAMET-S",2687290,"SV 90 PG 29 B-29","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",10,7.8317302370045585,{"$f":"F3523*(1-Elteq!$F$6)","v":7.8317302370045585}]
["ANAMET-S",2687360,"SV 90 PG 36 B-36","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",10,12.662690762796222,{"$f":"F3524*(1-Elteq!$F$6)","v":12.662690762796222}]
["ANAMET-S",2687480,"SV 90 PG 48 B-48","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",5,15.672750782712566,{"$f":"F3525*(1-Elteq!$F$6)","v":15.672750782712566}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},2688070,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",50,9.2903087034455045E-2,{"$f":"F3526*(1-Elteq!$F$6)","v":9.2903087034455045E-2}]
["ANAMET-S",2688100,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",50,9.2903087034455045E-2,{"$f":"F3527*(1-Elteq!$F$6)","v":9.2903087034455045E-2}]
["ANAMET-S",2688120,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",50,9.2903087034455045E-2,{"$f":"F3528*(1-Elteq!$F$6)","v":9.2903087034455045E-2}]
["ANAMET-S",2688130,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",50,9.2903087034455045E-2,{"$f":"F3529*(1-Elteq!$F$6)","v":9.2903087034455045E-2}]
["ANAMET-S",2688170,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",50,0.13935463055168257,{"$f":"F3530*(1-Elteq!$F$6)","v":0.13935463055168257}]
["ANAMET-S",2688180,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",50,0.13935463055168257,{"$f":"F3531*(1-Elteq!$F$6)","v":0.13935463055168257}]
["ANAMET-S",2688230,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",25,0.13935463055168257,{"$f":"F3532*(1-Elteq!$F$6)","v":0.13935463055168257}]
["ANAMET-S",2688290,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",20,0.18580617406891009,{"$f":"F3533*(1-Elteq!$F$6)","v":0.18580617406891009}]
["ANAMET-S",2688300,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",20,0.18580617406891009,{"$f":"F3534*(1-Elteq!$F$6)","v":0.18580617406891009}]
["ANAMET-S",2688370,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",10,0.18580617406891009,{"$f":"F3535*(1-Elteq!$F$6)","v":0.18580617406891009}]
["ANAMET-S",2688400,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",10,0.23225771758613761,{"$f":"F3536*(1-Elteq!$F$6)","v":0.23225771758613761}]
["ANAMET-S",2688500,"-","Fittings for Anaquick conduit, O-ring to obtain IP 68",5,0.23225771758613761,{"$f":"F3537*(1-Elteq!$F$6)","v":0.23225771758613761}]
["ANAMET-S",2651160,"MSV M16 B-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",30,11.687208348934446,{"$f":"F3538*(1-Elteq!$F$6)","v":11.687208348934446}]
["ANAMET-S",2651161,"MSV M16 B-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",30,10.851080565624349,{"$f":"F3539*(1-Elteq!$F$6)","v":10.851080565624349}]
["ANAMET-S",2651200,"MSV M20 B-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",30,13.684624720175229,{"$f":"F3540*(1-Elteq!$F$6)","v":13.684624720175229}]
["ANAMET-S",2651201,"MSV M20 B-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",30,12.523336132244539,{"$f":"F3541*(1-Elteq!$F$6)","v":12.523336132244539}]
["ANAMET-S",2651250,"MSV M25 B-23","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",30,19.528228894642449,{"$f":"F3542*(1-Elteq!$F$6)","v":19.528228894642449}]
["ANAMET-S",2651251,"MSV M25 B-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",30,14.595074973112887,{"$f":"F3543*(1-Elteq!$F$6)","v":14.595074973112887}]
["ANAMET-S",2651320,"MSV M32 B-29","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",20,24.535705285799576,{"$f":"F3544*(1-Elteq!$F$6)","v":24.535705285799576}]
["ANAMET-S",2651400,"MSV M40 B-37","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",10,40.654390886277525,{"$f":"F3545*(1-Elteq!$F$6)","v":40.654390886277525}]
["ANAMET-S",2651500,"MSV M50 B-48","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",10,47.408445313682407,{"$f":"F3546*(1-Elteq!$F$6)","v":47.408445313682407}]
["ANAMET-S",2651630,"MSV M63 B-48","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",10,58.426751435968782,{"$f":"F3547*(1-Elteq!$F$6)","v":58.426751435968782}]
["ANAMET-S",2653160,"MSV 90 M16 B-12","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",30,14.019075833499265,{"$f":"F3548*(1-Elteq!$F$6)","v":14.019075833499265}]
["ANAMET-S",2653161,"MSV 90 M16 B-10","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",30,14.019075833499265,{"$f":"F3549*(1-Elteq!$F$6)","v":14.019075833499265}]
["ANAMET-S",2653200,"MSV 90 M20 B-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",30,15.440493065126429,{"$f":"F3550*(1-Elteq!$F$6)","v":15.440493065126429}]
["ANAMET-S",2653201,"MSV 90 M20 B-12","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",30,14.019075833499265,{"$f":"F3551*(1-Elteq!$F$6)","v":14.019075833499265}]
["ANAMET-S",2653250,"MSV 90 M25 B-23","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",30,16.44384640509854,{"$f":"F3552*(1-Elteq!$F$6)","v":16.44384640509854}]
["ANAMET-S",2653251,"MSV 90 M25 B-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",30,22.278160270862323,{"$f":"F3553*(1-Elteq!$F$6)","v":22.278160270862323}]
["ANAMET-S",2653320,"MSV 90 M32 B-29","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",20,25.037381955785634,{"$f":"F3554*(1-Elteq!$F$6)","v":25.037381955785634}]
["ANAMET-S",2653400,"MSV 90 M40 B-36","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",10,45.578254499103643,{"$f":"F3555*(1-Elteq!$F$6)","v":45.578254499103643}]
["ANAMET-S",2653501,"MSV 90 M50 B-36","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",10,47.222639139613499,{"$f":"F3556*(1-Elteq!$F$6)","v":47.222639139613499}]
["ANAMET-S",2653630,"MSV 90 M63 B-48","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",10,71.869828129854412,{"$f":"F3557*(1-Elteq!$F$6)","v":71.869828129854412}]
["ANAMET-S",2655090,"MSV PG 9 B-10","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",30,10.851080565624349,{"$f":"F3558*(1-Elteq!$F$6)","v":10.851080565624349}]
["ANAMET-S",2655110,"MSV PG 11 B-12","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",30,12.523336132244539,{"$f":"F3559*(1-Elteq!$F$6)","v":12.523336132244539}]
["ANAMET-S",2655131,"MSV PG 13 B-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",30,13.684624720175229,{"$f":"F3560*(1-Elteq!$F$6)","v":13.684624720175229}]
["ANAMET-S",2655160,"MSV PG 16 B-17","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",30,14.595074973112887,{"$f":"F3561*(1-Elteq!$F$6)","v":14.595074973112887}]
["ANAMET-S",2655210,"MSV PG 21 B-23","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",30,22.036612244572733,{"$f":"F3562*(1-Elteq!$F$6)","v":22.036612244572733}]
["ANAMET-S",2655290,"MSV PG 29 B-29","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",20,24.535705285799576,{"$f":"F3563*(1-Elteq!$F$6)","v":24.535705285799576}]
["ANAMET-S",2655360,"MSV PG 36 B-36","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",10,42.6518072575183,{"$f":"F3564*(1-Elteq!$F$6)","v":42.6518072575183}]
["ANAMET-S",2655480,"MSV PG 48 B-48","Fittings for Anaquick conduit, Straight fixed with male thread IP 65/68",10,58.426751435968782,{"$f":"F3565*(1-Elteq!$F$6)","v":58.426751435968782}]
["ANAMET-S",2657090,"MSV 90 PG 9 B-10","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",30,14.019075833499265,{"$f":"F3566*(1-Elteq!$F$6)","v":14.019075833499265}]
["ANAMET-S",2657110,"MSV 90 PG 11 B-12","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",30,14.019075833499265,{"$f":"F3567*(1-Elteq!$F$6)","v":14.019075833499265}]
["ANAMET-S",2657130,"MSV 90 PG 13 B-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",30,15.440493065126429,{"$f":"F3568*(1-Elteq!$F$6)","v":15.440493065126429}]
["ANAMET-S",2657160,"MSV 90 PG 16 B-17","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",30,16.44384640509854,{"$f":"F3569*(1-Elteq!$F$6)","v":16.44384640509854}]
["ANAMET-S",2657210,"MSV 90 PG 21 B-23","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",30,22.278160270862323,{"$f":"F3570*(1-Elteq!$F$6)","v":22.278160270862323}]
["ANAMET-S",2657290,"MSV 90 PG 29 B-29","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",20,25.037381955785634,{"$f":"F3571*(1-Elteq!$F$6)","v":25.037381955785634}]
["ANAMET-S",2657360,"MSV 90 PG 36 B-36","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",10,47.166897287392828,{"$f":"F3572*(1-Elteq!$F$6)","v":47.166897287392828}]
["ANAMET-S",2657480,"MSV 90 PG 48 B-48","Fittings for Anaquick conduit, 90° elbow fixed male thread, IP 65/68",10,71.869828129854412,{"$f":"F3573*(1-Elteq!$F$6)","v":71.869828129854412}]
["ANAMET-S",2672070,"CH NW 7,5 G","Fittings for Anaquick conduit, Conduit holder",100,0.93832117904799595,{"$f":"F3574*(1-Elteq!$F$6)","v":0.93832117904799595}]
["ANAMET-S",2672100,"CH NW 10 G","Fittings for Anaquick conduit, Conduit holder",100,0.98477272256522352,{"$f":"F3575*(1-Elteq!$F$6)","v":0.98477272256522352}]
["ANAMET-S",2672120,"CH NW 12 G","Fittings for Anaquick conduit, Conduit holder",50,1.1334176618203515,{"$f":"F3576*(1-Elteq!$F$6)","v":1.1334176618203515}]
["ANAMET-S",2672170,"CH NW 17 G","Fittings for Anaquick conduit, Conduit holder",50,1.1891595140410245,{"$f":"F3577*(1-Elteq!$F$6)","v":1.1891595140410245}]
["ANAMET-S",2672230,"CH NW 23 G","Fittings for Anaquick conduit, Conduit holder",50,1.8301908145787644,{"$f":"F3578*(1-Elteq!$F$6)","v":1.8301908145787644}]
["ANAMET-S",2672290,"CH NW 29 G","Fittings for Anaquick conduit, Conduit holder",30,2.1181903843855747,{"$f":"F3579*(1-Elteq!$F$6)","v":2.1181903843855747}]
["ANAMET-S",2672360,"CH NW 37 G","Fittings for Anaquick conduit, Conduit holder",20,2.9543181676956705,{"$f":"F3580*(1-Elteq!$F$6)","v":2.9543181676956705}]
["ANAMET-S",2672480,"CH NW 50 G","Fittings for Anaquick conduit, Conduit holder",20,3.59534946823341,{"$f":"F3581*(1-Elteq!$F$6)","v":3.59534946823341}]
["ANAMET-S",2673070,"CH NW 7,5 B","Fittings for Anaquick conduit, Conduit holder",100,0.93832117904799595,{"$f":"F3582*(1-Elteq!$F$6)","v":0.93832117904799595}]
["ANAMET-S",2673100,"CH NW 10 B","Fittings for Anaquick conduit, Conduit holder",100,0.98477272256522352,{"$f":"F3583*(1-Elteq!$F$6)","v":0.98477272256522352}]
["ANAMET-S",2673120,"CH NW 12 B","Fittings for Anaquick conduit, Conduit holder",50,1.1334176618203515,{"$f":"F3584*(1-Elteq!$F$6)","v":1.1334176618203515}]
["ANAMET-S",2673170,"CH NW 17 B","Fittings for Anaquick conduit, Conduit holder",50,1.1891595140410245,{"$f":"F3585*(1-Elteq!$F$6)","v":1.1891595140410245}]
["ANAMET-S",2673230,"CH NW 23 B","Fittings for Anaquick conduit, Conduit holder",50,1.8301908145787644,{"$f":"F3586*(1-Elteq!$F$6)","v":1.8301908145787644}]
["ANAMET-S",2673290,"CH NW 29 B","Fittings for Anaquick conduit, Conduit holder",30,2.1181903843855747,{"$f":"F3587*(1-Elteq!$F$6)","v":2.1181903843855747}]
["ANAMET-S",2673360,"CH NW 37 B","Fittings for Anaquick conduit, Conduit holder",20,2.9543181676956705,{"$f":"F3588*(1-Elteq!$F$6)","v":2.9543181676956705}]
["ANAMET-S",2673480,"CH NW 50 B","Fittings for Anaquick conduit, Conduit holder",20,3.59534946823341,{"$f":"F3589*(1-Elteq!$F$6)","v":3.59534946823341}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},2674070,"CC NW 7,5 G","Fittings for Anaquick conduit, Conduit holder cover",100,0.59457975702051225,{"$f":"F3590*(1-Elteq!$F$6)","v":0.59457975702051225}]
["ANAMET-S",2674100,"CC NW 10 G","Fittings for Anaquick conduit, Conduit holder cover",50,0.59457975702051225,{"$f":"F3591*(1-Elteq!$F$6)","v":0.59457975702051225}]
["ANAMET-S",2674120,"CC NW 12 G","Fittings for Anaquick conduit, Conduit holder cover",50,0.68748284405496729,{"$f":"F3592*(1-Elteq!$F$6)","v":0.68748284405496729}]
["ANAMET-S",2674170,"CC NW 17 G","Fittings for Anaquick conduit, Conduit holder cover",50,0.68748284405496729,{"$f":"F3593*(1-Elteq!$F$6)","v":0.68748284405496729}]
["ANAMET-S",2674230,"CC NW 23 G","Fittings for Anaquick conduit, Conduit holder cover",50,0.8454180920135409,{"$f":"F3594*(1-Elteq!$F$6)","v":0.8454180920135409}]
["ANAMET-S",2674290,"CC NW 29 G","Fittings for Anaquick conduit, Conduit holder cover",30,0.8454180920135409,{"$f":"F3595*(1-Elteq!$F$6)","v":0.8454180920135409}]
["ANAMET-S",2674360,"CC NW 37 G","Fittings for Anaquick conduit, Conduit holder cover",20,0.93832117904799595,{"$f":"F3596*(1-Elteq!$F$6)","v":0.93832117904799595}]
["ANAMET-S",2674480,"CC NW 50 G","Fittings for Anaquick conduit, Conduit holder cover",20,0.93832117904799595,{"$f":"F3597*(1-Elteq!$F$6)","v":0.93832117904799595}]
["ANAMET-S",2675000,"CH CON - G","Fittings for Anaquick conduit, Conduit holder cover",100,0.20438679147580111,{"$f":"F3598*(1-Elteq!$F$6)","v":0.20438679147580111}]
["ANAMET-S",2675010,"CH CON - B","Fittings for Anaquick conduit, Conduit holder cover",100,0.20438679147580111,{"$f":"F3599*(1-Elteq!$F$6)","v":0.20438679147580111}]
["ANAMET-S",2675070,"CC NW 7,5 B","Fittings for Anaquick conduit, Conduit holder cover",100,0.59457975702051225,{"$f":"F3600*(1-Elteq!$F$6)","v":0.59457975702051225}]
["ANAMET-S",2675100,"CC NW 10 B","Fittings for Anaquick conduit, Conduit holder cover",100,0.59457975702051225,{"$f":"F3601*(1-Elteq!$F$6)","v":0.59457975702051225}]
["ANAMET-S",2675120,"CC NW 12 B","Fittings for Anaquick conduit, Conduit holder cover",50,0.68748284405496729,{"$f":"F3602*(1-Elteq!$F$6)","v":0.68748284405496729}]
["ANAMET-S",2675170,"CC NW 17 B","Fittings for Anaquick conduit, Conduit holder cover",50,0.68748284405496729,{"$f":"F3603*(1-Elteq!$F$6)","v":0.68748284405496729}]
["ANAMET-S",2675230,"CC NW 23 B","Fittings for Anaquick conduit, Conduit holder cover",50,0.8454180920135409,{"$f":"F3604*(1-Elteq!$F$6)","v":0.8454180920135409}]
["ANAMET-S",2675290,"CC NW 29 B","Fittings for Anaquick conduit, Conduit holder cover",30,0.8454180920135409,{"$f":"F3605*(1-Elteq!$F$6)","v":0.8454180920135409}]
["ANAMET-S",2675360,"CC NW 37 B","Fittings for Anaquick conduit, Conduit holder cover",20,0.93832117904799595,{"$f":"F3606*(1-Elteq!$F$6)","v":0.93832117904799595}]
["ANAMET-S",2675480,"CC NW 50 B","Fittings for Anaquick conduit, Conduit holder cover",20,0.93832117904799595,{"$f":"F3607*(1-Elteq!$F$6)","v":0.93832117904799595}]
["ANAMET-S",2676100,"CLIP NW 10 B","Fittings for Anaquick conduit, Conduit clip",500,5.3790887392949465,{"$f":"F3608*(1-Elteq!$F$6)","v":5.3790887392949465}]
["ANAMET-S",2676130,"CLIP NW 13 B","Fittings for Anaquick conduit, Conduit clip",500,5.5184433698466293,{"$f":"F3609*(1-Elteq!$F$6)","v":5.5184433698466293}]
["ANAMET-S",2676170,"CLIP NW 17 B","Fittings for Anaquick conduit, Conduit clip",500,5.78786232224655,{"$f":"F3610*(1-Elteq!$F$6)","v":5.78786232224655}]
["ANAMET-S",2676220,"CLIP NW 22 B","Fittings for Anaquick conduit, Conduit clip",500,5.9086363353913409,{"$f":"F3611*(1-Elteq!$F$6)","v":5.9086363353913409}]
["ANAMET-S",2677100,"NW 10","Fittings for Anaquick conduit, Conduit reducer",2000,0.23225771758613761,{"$f":"F3612*(1-Elteq!$F$6)","v":0.23225771758613761}]
["ANAMET-S",2677110,"NW 10","Fittings for Anaquick conduit, Conduit reducer",2000,0.24154802628958311,{"$f":"F3613*(1-Elteq!$F$6)","v":0.24154802628958311}]
["ANAMET-S",2677130,"NW 13","Fittings for Anaquick conduit, Conduit reducer",2000,0.24154802628958311,{"$f":"F3614*(1-Elteq!$F$6)","v":0.24154802628958311}]
["ANAMET-S",2677140,"NW 13","Fittings for Anaquick conduit, Conduit reducer",500,0.2508383349930286,{"$f":"F3615*(1-Elteq!$F$6)","v":0.2508383349930286}]
["ANAMET-S",2677170,"NW 17","Fittings for Anaquick conduit, Conduit reducer",500,0.31587049591714716,{"$f":"F3616*(1-Elteq!$F$6)","v":0.31587049591714716}]
["ANAMET-S",2678170,"NW 17","Fittings for Anaquick conduit, Conduit reducer",500,0.19509648277235556,{"$f":"F3617*(1-Elteq!$F$6)","v":0.19509648277235556}]
["ANAMET-S",2678200,"NW 22","Fittings for Anaquick conduit, Conduit reducer",1000,0.22296740888269209,{"$f":"F3618*(1-Elteq!$F$6)","v":0.22296740888269209}]
["ANAMET-S",2678210,"NW 22","Fittings for Anaquick conduit, Conduit reducer",1000,0.3344511133240381,{"$f":"F3619*(1-Elteq!$F$6)","v":0.3344511133240381}]
["ANAMET-S",2678220,"NW 22","Fittings for Anaquick conduit, Conduit reducer",1000,0.74322469627564036,{"$f":"F3620*(1-Elteq!$F$6)","v":0.74322469627564036}]
["ANAMET-S",7977010,"T 7-7-7","Fittings for Anaquick conduit, T-joint splitable, IP 40",500,0.44593481776538418,{"$f":"F3621*(1-Elteq!$F$6)","v":0.44593481776538418}]
["ANAMET-S",7977020,"T 10-7-7","Fittings for Anaquick conduit, T-joint splitable, IP 40",500,0.8268374746066498,{"$f":"F3622*(1-Elteq!$F$6)","v":0.8268374746066498}]
["ANAMET-S",7977030,"T 10-10-7","Fittings for Anaquick conduit, T-joint splitable, IP 40",500,0.39948327424815672,{"$f":"F3623*(1-Elteq!$F$6)","v":0.39948327424815672}]
["ANAMET-S",7977040,"T 10-10-10","Fittings for Anaquick conduit, T-joint splitable, IP 40",500,0.39948327424815672,{"$f":"F3624*(1-Elteq!$F$6)","v":0.39948327424815672}]
["ANAMET-S",7977050,"T 12-12-7","Fittings for Anaquick conduit, T-joint splitable, IP 40",500,0.43664450906193863,{"$f":"F3625*(1-Elteq!$F$6)","v":0.43664450906193863}]
["ANAMET-S",7977060,"T 12-10-10","Fittings for Anaquick conduit, T-joint splitable, IP 40",500,0.65032160924118521,{"$f":"F3626*(1-Elteq!$F$6)","v":0.65032160924118521}]
["ANAMET-S",7977070,"T 17-10-17","Fittings for Anaquick conduit, T-joint splitable, IP 40",500,0.5016766699860572,{"$f":"F3627*(1-Elteq!$F$6)","v":0.5016766699860572}]
["ANAMET-S",7977080,"T 17-12-12","Fittings for Anaquick conduit, T-joint splitable, IP 40",500,0.5202572873929483,{"$f":"F3628*(1-Elteq!$F$6)","v":0.5202572873929483}]
["ANAMET-S",7977090,"T 17-12-17","Fittings for Anaquick conduit, T-joint splitable, IP 40",250,0.56670883091017576,{"$f":"F3629*(1-Elteq!$F$6)","v":0.56670883091017576}]
["ANAMET-S",7977100,"T 17-23-17","Fittings for Anaquick conduit, T-joint splitable, IP 40",250,0.68748284405496729,{"$f":"F3630*(1-Elteq!$F$6)","v":0.68748284405496729}]
["ANAMET-S",7977110,"T 23-10-23","Fittings for Anaquick conduit, T-joint splitable, IP 40",250,1.7001264927305273,{"$f":"F3631*(1-Elteq!$F$6)","v":1.7001264927305273}]
["ANAMET-S",7977120,"T 23-12-23","Fittings for Anaquick conduit, T-joint splitable, IP 40",500,0.8454180920135409,{"$f":"F3632*(1-Elteq!$F$6)","v":0.8454180920135409}]
["ANAMET-S",7977130,"T 23-17-12","Fittings for Anaquick conduit, T-joint splitable, IP 40",250,0.71535377016530377,{"$f":"F3633*(1-Elteq!$F$6)","v":0.71535377016530377}]
["ANAMET-S",7977140,"T 23-23-10","Fittings for Anaquick conduit, T-joint splitable, IP 40",100,0.81754716590320442,{"$f":"F3634*(1-Elteq!$F$6)","v":0.81754716590320442}]
["ANAMET-S",7977150,"T 23-23-23","Fittings for Anaquick conduit, T-joint splitable, IP 40",500,1.3749656881099346,{"$f":"F3635*(1-Elteq!$F$6)","v":1.3749656881099346}]
["ANAMET-S",7978010,"Y 12-10-10","Fittings for Anaquick conduit, Y-joint splitable, IP 40",500,0.91974056164110485,{"$f":"F3636*(1-Elteq!$F$6)","v":0.91974056164110485}]
["ANAMET-S",7978020,"Y 12-10-12","Fittings for Anaquick conduit, Y-joint splitable, IP 40",500,0.91974056164110485,{"$f":"F3637*(1-Elteq!$F$6)","v":0.91974056164110485}]
["ANAMET-S",7978030,"Y 12-12-12","Fittings for Anaquick conduit, Y-joint splitable, IP 40",500,0.91974056164110485,{"$f":"F3638*(1-Elteq!$F$6)","v":0.91974056164110485}]
["ANAMET-S",7978040,"Y 17-10-10","Fittings for Anaquick conduit, Y-joint splitable, IP 40",500,0.6781925353515218,{"$f":"F3639*(1-Elteq!$F$6)","v":0.6781925353515218}]
["ANAMET-S",7978050,"Y 17-10-17","Fittings for Anaquick conduit, Y-joint splitable, IP 40",500,0.78038593108942222,{"$f":"F3640*(1-Elteq!$F$6)","v":0.78038593108942222}]
["ANAMET-S",7978060,"Y 17-12-10","Fittings for Anaquick conduit, Y-joint splitable, IP 40",500,1.0219339573790056,{"$f":"F3641*(1-Elteq!$F$6)","v":1.0219339573790056}]
["ANAMET-S",7978070,"Y 17-12-12","Fittings for Anaquick conduit, Y-joint splitable, IP 40",500,0.69677315275841278,{"$f":"F3642*(1-Elteq!$F$6)","v":0.69677315275841278}]
["ANAMET-S",7978080,"Y 17-17-10","Fittings for Anaquick conduit, Y-joint splitable, IP 40",500,1.0219339573790056,{"$f":"F3643*(1-Elteq!$F$6)","v":1.0219339573790056}]
["ANAMET-S",7978090,"Y 23-10-23","Fittings for Anaquick conduit, Y-joint splitable, IP 40",100,1.1055467357100148,{"$f":"F3644*(1-Elteq!$F$6)","v":1.1055467357100148}]
["ANAMET-S",7978100,"Y 23-12-23","Fittings for Anaquick conduit, Y-joint splitable, IP 40",100,1.0683855008962329,{"$f":"F3645*(1-Elteq!$F$6)","v":1.0683855008962329}]
["ANAMET-S",7978110,"Y 23-23-23","Fittings for Anaquick conduit, Y-joint splitable, IP 40",250,1.1705788966341335,{"$f":"F3646*(1-Elteq!$F$6)","v":1.1705788966341335}]
["ANAMET-S",7998010,"T 10-10-10","Fittings for Anaquick conduit, T-joint conduit",100,0.68748284405496729,{"$f":"F3647*(1-Elteq!$F$6)","v":0.68748284405496729}]
["ANAMET-S",7998020,"T 17-17-10","Fittings for Anaquick conduit, T-joint conduit",100,0.46451543517227523,{"$f":"F3648*(1-Elteq!$F$6)","v":0.46451543517227523}]
["ANAMET-S",7998030,"T 17-17-17","Fittings for Anaquick conduit, T-joint conduit",100,0.91974056164110485,{"$f":"F3649*(1-Elteq!$F$6)","v":0.91974056164110485}]
["ANAMET-S",7998040,"T 23-23-10","Fittings for Anaquick conduit, T-joint conduit",100,1.4585784664409442,{"$f":"F3650*(1-Elteq!$F$6)","v":1.4585784664409442}]
["ANAMET-S",7998050,"T 23-23-17","Fittings for Anaquick conduit, T-joint conduit",100,1.8766423580959919,{"$f":"F3651*(1-Elteq!$F$6)","v":1.8766423580959919}]
["ANAMET-S",7998060,"T 23-23-23","Fittings for Anaquick conduit, T-joint conduit",250,1.4585784664409442,{"$f":"F3652*(1-Elteq!$F$6)","v":1.4585784664409442}]
["ANAMET-S",7998070,"T 10-17-23","Fittings for Anaquick conduit, T-joint conduit",100,1.2820626010754794,{"$f":"F3653*(1-Elteq!$F$6)","v":1.2820626010754794}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},2699070,"CN 7 G","Fittings for Anaquick conduit, Locknut, polyamide",50,0.13006432184823707,{"$f":"F3654*(1-Elteq!$F$6)","v":0.13006432184823707}]
["ANAMET-S",2699073,"CN 7 B","Fittings for Anaquick conduit, Locknut, polyamide",50,0.13006432184823707,{"$f":"F3655*(1-Elteq!$F$6)","v":0.13006432184823707}]
["ANAMET-S",2699090,"CN 9 G","Fittings for Anaquick conduit, Locknut, polyamide",50,0.13006432184823707,{"$f":"F3656*(1-Elteq!$F$6)","v":0.13006432184823707}]
["ANAMET-S",2699093,"CN 9 B","Fittings for Anaquick conduit, Locknut, polyamide",50,0.13006432184823707,{"$f":"F3657*(1-Elteq!$F$6)","v":0.13006432184823707}]
["ANAMET-S",2699110,"CN 11 G","Fittings for Anaquick conduit, Locknut, polyamide",50,0.13006432184823707,{"$f":"F3658*(1-Elteq!$F$6)","v":0.13006432184823707}]
["ANAMET-S",2699113,"CN 11 B","Fittings for Anaquick conduit, Locknut, polyamide",50,0.13006432184823707,{"$f":"F3659*(1-Elteq!$F$6)","v":0.13006432184823707}]
["ANAMET-S",2699130,"CN 13 G","Fittings for Anaquick conduit, Locknut, polyamide",50,0.18580617406891009,{"$f":"F3660*(1-Elteq!$F$6)","v":0.18580617406891009}]
["ANAMET-S",2699133,"CN 13 B","Fittings for Anaquick conduit, Locknut, polyamide",50,0.18580617406891009,{"$f":"F3661*(1-Elteq!$F$6)","v":0.18580617406891009}]
["ANAMET-S",2699160,"CN 16 G","Fittings for Anaquick conduit, Locknut, polyamide",50,0.18580617406891009,{"$f":"F3662*(1-Elteq!$F$6)","v":0.18580617406891009}]
["ANAMET-S",2699163,"CN 16 B","Fittings for Anaquick conduit, Locknut, polyamide",20,0.18580617406891009,{"$f":"F3663*(1-Elteq!$F$6)","v":0.18580617406891009}]
["ANAMET-S",2699210,"CN 21 G","Fittings for Anaquick conduit, Locknut, polyamide",20,0.3344511133240381,{"$f":"F3664*(1-Elteq!$F$6)","v":0.3344511133240381}]
["ANAMET-S",2699213,"CN 21 B","Fittings for Anaquick conduit, Locknut, polyamide",20,0.3344511133240381,{"$f":"F3665*(1-Elteq!$F$6)","v":0.3344511133240381}]
["ANAMET-S",2699290,"CN 29 G","Fittings for Anaquick conduit, Locknut, polyamide",20,0.59457975702051225,{"$f":"F3666*(1-Elteq!$F$6)","v":0.59457975702051225}]
["ANAMET-S",2699293,"CN 29 B","Fittings for Anaquick conduit, Locknut, polyamide",20,0.59457975702051225,{"$f":"F3667*(1-Elteq!$F$6)","v":0.59457975702051225}]
["ANAMET-S",2699360,"CN 36 G","Fittings for Anaquick conduit, Locknut, polyamide",10,1.2541916749651432,{"$f":"F3668*(1-Elteq!$F$6)","v":1.2541916749651432}]
["ANAMET-S",2699363,"CN 36 B","Fittings for Anaquick conduit, Locknut, polyamide",10,1.2541916749651432,{"$f":"F3669*(1-Elteq!$F$6)","v":1.2541916749651432}]
["ANAMET-S",2699480,"CN 48 G","Fittings for Anaquick conduit, Locknut, polyamide",5,1.8859326667994372,{"$f":"F3670*(1-Elteq!$F$6)","v":1.8859326667994372}]
["ANAMET-S",2699483,"CN 48 B","Fittings for Anaquick conduit, Locknut, polyamide",5,1.8859326667994372,{"$f":"F3671*(1-Elteq!$F$6)","v":1.8859326667994372}]
["ANAMET-S",7983120,"CN M 12 G","Fittings for Anaquick conduit, Locknut, polyamide",50,0.13006432184823707,{"$f":"F3672*(1-Elteq!$F$6)","v":0.13006432184823707}]
["ANAMET-S",7983123,"CN M 12 B","Fittings for Anaquick conduit, Locknut, polyamide",50,0.13006432184823707,{"$f":"F3673*(1-Elteq!$F$6)","v":0.13006432184823707}]
["ANAMET-S",7983160,"CN M 16 G","Fittings for Anaquick conduit, Locknut, polyamide",50,0.18580617406891009,{"$f":"F3674*(1-Elteq!$F$6)","v":0.18580617406891009}]
["ANAMET-S",7983163,"CN M 16 B","Fittings for Anaquick conduit, Locknut, polyamide",50,0.18580617406891009,{"$f":"F3675*(1-Elteq!$F$6)","v":0.18580617406891009}]
["ANAMET-S",7983200,"CN M 20 G","Fittings for Anaquick conduit, Locknut, polyamide",50,0.18580617406891009,{"$f":"F3676*(1-Elteq!$F$6)","v":0.18580617406891009}]
["ANAMET-S",7983203,"CN M 20 B","Fittings for Anaquick conduit, Locknut, polyamide",50,0.18580617406891009,{"$f":"F3677*(1-Elteq!$F$6)","v":0.18580617406891009}]
["ANAMET-S",7983250,"CN M 25 G","Fittings for Anaquick conduit, Locknut, polyamide",50,0.26012864369647415,{"$f":"F3678*(1-Elteq!$F$6)","v":0.26012864369647415}]
["ANAMET-S",7983253,"CN M 25 B","Fittings for Anaquick conduit, Locknut, polyamide",50,0.26012864369647415,{"$f":"F3679*(1-Elteq!$F$6)","v":0.26012864369647415}]
["ANAMET-S",7983320,"CN M 32 G","Fittings for Anaquick conduit, Locknut, polyamide",50,0.5016766699860572,{"$f":"F3680*(1-Elteq!$F$6)","v":0.5016766699860572}]
["ANAMET-S",7983323,"CN M 32 B","Fittings for Anaquick conduit, Locknut, polyamide",50,0.5016766699860572,{"$f":"F3681*(1-Elteq!$F$6)","v":0.5016766699860572}]
["ANAMET-S",7983400,"CN M 40 G","Fittings for Anaquick conduit, Locknut, polyamide",20,0.80825685719975882,{"$f":"F3682*(1-Elteq!$F$6)","v":0.80825685719975882}]
["ANAMET-S",7983403,"CN M 40 B","Fittings for Anaquick conduit, Locknut, polyamide",20,0.80825685719975882,{"$f":"F3683*(1-Elteq!$F$6)","v":0.80825685719975882}]
["ANAMET-S",7983500,"CN M 50 G","Fittings for Anaquick conduit, Locknut, polyamide",10,1.3285141445927069,{"$f":"F3684*(1-Elteq!$F$6)","v":1.3285141445927069}]
["ANAMET-S",7983503,"CN M 50 B","Fittings for Anaquick conduit, Locknut, polyamide",10,1.3285141445927069,{"$f":"F3685*(1-Elteq!$F$6)","v":1.3285141445927069}]
["ANAMET-S",7983630,"CN M 63 G","Fittings for Anaquick conduit, Locknut, polyamide",5,1.9881260625373383,{"$f":"F3686*(1-Elteq!$F$6)","v":1.9881260625373383}]
["ANAMET-S",7983633,"CN M 63 B","Fittings for Anaquick conduit, Locknut, polyamide",5,1.9881260625373383,{"$f":"F3687*(1-Elteq!$F$6)","v":1.9881260625373383}]
["ANAMET-S",2661090,"PG 9","Fittings for Anaquick conduit, Reducer Pg/PG polyamide",100,0.91045025293765935,{"$f":"F3688*(1-Elteq!$F$6)","v":0.91045025293765935}]
["ANAMET-S",2661110,"PG 11","Fittings for Anaquick conduit, Reducer Pg/PG polyamide",100,0.863998709420432,{"$f":"F3689*(1-Elteq!$F$6)","v":0.863998709420432}]
["ANAMET-S",2661150,"PG16","Fittings for Anaquick conduit, Reducer Pg/PG polyamide",100,1.1148370444134605,{"$f":"F3690*(1-Elteq!$F$6)","v":1.1148370444134605}]
["ANAMET-S",2661160,"PG 16","Fittings for Anaquick conduit, Reducer Pg/PG polyamide",100,1.0219339573790056,{"$f":"F3691*(1-Elteq!$F$6)","v":1.0219339573790056}]
["ANAMET-S",2661210,"PG 21","Fittings for Anaquick conduit, Reducer Pg/PG polyamide",100,1.514320318661617,{"$f":"F3692*(1-Elteq!$F$6)","v":1.514320318661617}]
["ANAMET-S",2661290,"PG 29","Fittings for Anaquick conduit, Reducer Pg/PG polyamide",50,3.1029631069507984,{"$f":"F3693*(1-Elteq!$F$6)","v":3.1029631069507984}]
["ANAMET-S",2661360,"PG 36","Fittings for Anaquick conduit, Reducer Pg/PG polyamide",50,3.4467045289782821,{"$f":"F3694*(1-Elteq!$F$6)","v":3.4467045289782821}]
["ANAMET-S",2661420,"PG 42","Fittings for Anaquick conduit, Reducer Pg/PG polyamide",25,7.7109562238597684,{"$f":"F3695*(1-Elteq!$F$6)","v":7.7109562238597684}]
["ANAMET-S",2661480,"PG 48","Fittings for Anaquick conduit, Reducer Pg/PG polyamide",25,9.6526307428798805,{"$f":"F3696*(1-Elteq!$F$6)","v":9.6526307428798805}]
["ANAMET-S",2662070,"PG 7","Fittings for Anaquick conduit, Enlarger Pg/PG polyamide",100,0.6781925353515218,{"$f":"F3697*(1-Elteq!$F$6)","v":0.6781925353515218}]
["ANAMET-S",2662090,"PG 9","Fittings for Anaquick conduit, Enlarger Pg/PG polyamide",100,0.78038593108942222,{"$f":"F3698*(1-Elteq!$F$6)","v":0.78038593108942222}]
["ANAMET-S",2662110,"PG 11","Fittings for Anaquick conduit, Enlarger Pg/PG polyamide",100,0.92903087034455045,{"$f":"F3699*(1-Elteq!$F$6)","v":0.92903087034455045}]
["ANAMET-S",2662160,"PG 16","Fittings for Anaquick conduit, Enlarger Pg/PG polyamide",100,1.514320318661617,{"$f":"F3700*(1-Elteq!$F$6)","v":1.514320318661617}]
["ANAMET-S",2662210,"PG 21","Fittings for Anaquick conduit, Enlarger Pg/PG polyamide",50,3.1308340330611348,{"$f":"F3701*(1-Elteq!$F$6)","v":3.1308340330611348}]
["ANAMET-S",2662290,"PG29","Fittings for Anaquick conduit, Enlarger Pg/PG polyamide",25,5.4998627524397383,{"$f":"F3702*(1-Elteq!$F$6)","v":5.4998627524397383}]
["ANAMET-S",2662360,"PG 36","Fittings for Anaquick conduit, Enlarger Pg/PG polyamide",10,8.110439498107926,{"$f":"F3703*(1-Elteq!$F$6)","v":8.110439498107926}]
["ANAMET-S",2662420,"PG 42","Fittings for Anaquick conduit, Enlarger Pg/PG polyamide",10,10.609532539334765,{"$f":"F3704*(1-Elteq!$F$6)","v":10.609532539334765}]
["ANAMET-S",2664160,"M16","Fittings for Anaquick conduit, Reducer ISO/ISO polyamide",50,0.57599913961362126,{"$f":"F3705*(1-Elteq!$F$6)","v":0.57599913961362126}]
["ANAMET-S",2664200,"M20","Fittings for Anaquick conduit, Reducer ISO/ISO polyamide",50,0.61316037442740334,{"$f":"F3706*(1-Elteq!$F$6)","v":0.61316037442740334}]
["ANAMET-S",2664250,"M25","Fittings for Anaquick conduit, Reducer ISO/ISO polyamide",20,0.68748284405496729,{"$f":"F3707*(1-Elteq!$F$6)","v":0.68748284405496729}]
["ANAMET-S",2664320,"M32","Fittings for Anaquick conduit, Reducer ISO/ISO polyamide",20,0.863998709420432,{"$f":"F3708*(1-Elteq!$F$6)","v":0.863998709420432}]
["ANAMET-S",2664400,"M40","Fittings for Anaquick conduit, Reducer ISO/ISO polyamide",20,1.3563850707030436,{"$f":"F3709*(1-Elteq!$F$6)","v":1.3563850707030436}]
["ANAMET-S",2664500,"M50","Fittings for Anaquick conduit, Reducer ISO/ISO polyamide",10,2.8707053893646606,{"$f":"F3710*(1-Elteq!$F$6)","v":2.8707053893646606}]
["ANAMET-S",2664630,"M63","Fittings for Anaquick conduit, Reducer ISO/ISO polyamide",5,3.502446381198955,{"$f":"F3711*(1-Elteq!$F$6)","v":3.502446381198955}]
["ANAMET-S",2665120,"M12","Fittings for Anaquick conduit, Enlarger ISO/ISO polyamide",50,0.62245068313084884,{"$f":"F3712*(1-Elteq!$F$6)","v":0.62245068313084884}]
["ANAMET-S",2665160,"M16","Fittings for Anaquick conduit, Enlarger ISO/ISO polyamide",50,0.75251500497908597,{"$f":"F3713*(1-Elteq!$F$6)","v":0.75251500497908597}]
["ANAMET-S",2665200,"M20","Fittings for Anaquick conduit, Enlarger ISO/ISO polyamide",50,0.78038593108942222,{"$f":"F3714*(1-Elteq!$F$6)","v":0.78038593108942222}]
["ANAMET-S",2665250,"M25","Fittings for Anaquick conduit, Enlarger ISO/ISO polyamide",20,0.87328901812387727,{"$f":"F3715*(1-Elteq!$F$6)","v":0.87328901812387727}]
["ANAMET-S",2665320,"M32","Fittings for Anaquick conduit, Enlarger ISO/ISO polyamide",20,1.2727722923720342,{"$f":"F3716*(1-Elteq!$F$6)","v":1.2727722923720342}]
["ANAMET-S",2665400,"M40","Fittings for Anaquick conduit, Enlarger ISO/ISO polyamide",20,2.5176736586337318,{"$f":"F3717*(1-Elteq!$F$6)","v":2.5176736586337318}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},2665500,"M50","Fittings for Anaquick conduit, Enlarger ISO/ISO polyamide",10,3.483865763792064,{"$f":"F3718*(1-Elteq!$F$6)","v":3.483865763792064}]
["ANAMET-S",2666120,"M12","Fittings for Anaquick conduit, Blindplug ISO polyamide",50,0.27870926110336514,{"$f":"F3719*(1-Elteq!$F$6)","v":0.27870926110336514}]
["ANAMET-S",2666160,"M16","Fittings for Anaquick conduit, Blindplug ISO polyamide",50,0.31587049591714716,{"$f":"F3720*(1-Elteq!$F$6)","v":0.31587049591714716}]
["ANAMET-S",2666200,"M20","Fittings for Anaquick conduit, Blindplug ISO polyamide",50,0.37161234813782018,{"$f":"F3721*(1-Elteq!$F$6)","v":0.37161234813782018}]
["ANAMET-S",2666250,"M25","Fittings for Anaquick conduit, Blindplug ISO polyamide",20,0.46451543517227523,{"$f":"F3722*(1-Elteq!$F$6)","v":0.46451543517227523}]
["ANAMET-S",2666320,"M32","Fittings for Anaquick conduit, Blindplug ISO polyamide",20,0.87328901812387727,{"$f":"F3723*(1-Elteq!$F$6)","v":0.87328901812387727}]
["ANAMET-S",2666400,"M40","Fittings for Anaquick conduit, Blindplug ISO polyamide",20,1.0869661183031241,{"$f":"F3724*(1-Elteq!$F$6)","v":1.0869661183031241}]
["ANAMET-S",2666500,"M50","Fittings for Anaquick conduit, Blindplug ISO polyamide",10,1.8952229755028829,{"$f":"F3725*(1-Elteq!$F$6)","v":1.8952229755028829}]
["ANAMET-S",2666630,"M63","Fittings for Anaquick conduit, Blindplug ISO polyamide",5,2.7870926110336511,{"$f":"F3726*(1-Elteq!$F$6)","v":2.7870926110336511}]
["ANAMET-S",2667070,"PG 7","Fittings for Anaquick conduit, Blindplug PG polyamide",50,0.73393438757219487,{"$f":"F3727*(1-Elteq!$F$6)","v":0.73393438757219487}]
["ANAMET-S",2667090,"PG 9","Fittings for Anaquick conduit, Blindplug PG polyamide",50,0.73393438757219487,{"$f":"F3728*(1-Elteq!$F$6)","v":0.73393438757219487}]
["ANAMET-S",2667110,"PG 11","Fittings for Anaquick conduit, Blindplug PG polyamide",50,0.80825685719975882,{"$f":"F3729*(1-Elteq!$F$6)","v":0.80825685719975882}]
["ANAMET-S",2667130,"PG13,5","Fittings for Anaquick conduit, Blindplug PG polyamide",50,0.85470840071698639,{"$f":"F3730*(1-Elteq!$F$6)","v":0.85470840071698639}]
["ANAMET-S",2667160,"PG 16","Fittings for Anaquick conduit, Blindplug PG polyamide",20,0.93832117904799595,{"$f":"F3731*(1-Elteq!$F$6)","v":0.93832117904799595}]
["ANAMET-S",2667210,"PG 21","Fittings for Anaquick conduit, Blindplug PG polyamide",20,1.2913529097789249,{"$f":"F3732*(1-Elteq!$F$6)","v":1.2913529097789249}]
["ANAMET-S",2667290,"PG29","Fittings for Anaquick conduit, Blindplug PG polyamide",20,2.378319028082049,{"$f":"F3733*(1-Elteq!$F$6)","v":2.378319028082049}]
["ANAMET-S",2667360,"PG 36","Fittings for Anaquick conduit, Blindplug PG polyamide",10,5.1839922565225915,{"$f":"F3734*(1-Elteq!$F$6)","v":5.1839922565225915}]
["ANAMET-S",2667480,"PG 48","Fittings for Anaquick conduit, Blindplug PG polyamide",5,7.032763688508247,{"$f":"F3735*(1-Elteq!$F$6)","v":7.032763688508247}]
["ANAMET-S",3010701,"GIG NW 70 PA 6 G","PA6 gigant conduit grey, Corrugated nylon conduit, IP 67",10,22.705514471220813,{"$f":"F3736*(1-Elteq!$F$6)","v":22.705514471220813}]
["ANAMET-S",3010703,"GIG NW 70 PA 6 G","PA6 gigant conduit grey, Corrugated nylon conduit, IP 67",25,22.705514471220813,{"$f":"F3737*(1-Elteq!$F$6)","v":22.705514471220813}]
["ANAMET-S",3010991,"GIG NW 95 PA 6 G","PA6 gigant conduit grey, Corrugated nylon conduit, IP 67",10,28.437634941246685,{"$f":"F3738*(1-Elteq!$F$6)","v":28.437634941246685}]
["ANAMET-S",3010993,"GIG NW 95 PA 6 G","PA6 gigant conduit grey, Corrugated nylon conduit, IP 67",25,28.437634941246685,{"$f":"F3739*(1-Elteq!$F$6)","v":28.437634941246685}]
["ANAMET-S",3011701,"GIG NW 70 PA 6 B","PA6 gigant conduit black, Corrugated nylon conduit, IP 67",10,22.705514471220813,{"$f":"F3740*(1-Elteq!$F$6)","v":22.705514471220813}]
["ANAMET-S",3011703,"GIG NW 70 PA 6 B","PA6 gigant conduit black, Corrugated nylon conduit, IP 67",25,22.705514471220813,{"$f":"F3741*(1-Elteq!$F$6)","v":22.705514471220813}]
["ANAMET-S",3011991,"GIG NW 95 PA 6 B","PA6 gigant conduit black, Corrugated nylon conduit, IP 67",10,28.437634941246685,{"$f":"F3742*(1-Elteq!$F$6)","v":28.437634941246685}]
["ANAMET-S",3011993,"GIG NW 95 PA 6 B","PA6 gigant conduit black, Corrugated nylon conduit, IP 67",25,28.437634941246685,{"$f":"F3743*(1-Elteq!$F$6)","v":28.437634941246685}]
["ANAMET-S",3012701,"GIG NW 70 PP G","PP gigant conduit grey, Corrugated nylon conduit, IP 67",10,15.700621708822899,{"$f":"F3744*(1-Elteq!$F$6)","v":15.700621708822899}]
["ANAMET-S",3012703,"GIG NW 70 PP G","PP gigant conduit grey, Corrugated nylon conduit, IP 67",25,15.700621708822899,{"$f":"F3745*(1-Elteq!$F$6)","v":15.700621708822899}]
["ANAMET-S",3012991,"GIG NW 95 PP G","PP gigant conduit grey, Corrugated nylon conduit, IP 67",10,24.637898681537475,{"$f":"F3746*(1-Elteq!$F$6)","v":24.637898681537475}]
["ANAMET-S",3012993,"GIG NW 95 PP G","PP gigant conduit grey, Corrugated nylon conduit, IP 67",25,24.637898681537475,{"$f":"F3747*(1-Elteq!$F$6)","v":24.637898681537475}]
["ANAMET-S",3013701,"GIG NW 70 PP B","PP gigant conduit black, Corrugated nylon conduit, IP 67",10,12.718432615016894,{"$f":"F3748*(1-Elteq!$F$6)","v":12.718432615016894}]
["ANAMET-S",3013703,"GIG NW 70 PP B","PP gigant conduit black, Corrugated nylon conduit, IP 67",25,12.718432615016894,{"$f":"F3749*(1-Elteq!$F$6)","v":12.718432615016894}]
["ANAMET-S",3013991,"GIG NW 95 PP B","PP gigant conduit black, Corrugated nylon conduit, IP 67",10,19.751196303525145,{"$f":"F3750*(1-Elteq!$F$6)","v":19.751196303525145}]
["ANAMET-S",3013993,"GIG NW 95 PP B","PP gigant conduit black, Corrugated nylon conduit, IP 67",25,19.751196303525145,{"$f":"F3751*(1-Elteq!$F$6)","v":19.751196303525145}]
["ANAMET-S",2690703,"70 mm","Fittings for gigant conduit, Straight fixed with flange, IP 54",70,20.801001187014485,{"$f":"F3752*(1-Elteq!$F$6)","v":20.801001187014485}]
["ANAMET-S",2690993,"95 mm","Fittings for gigant conduit, Straight fixed with flange, IP 54",50,25.436865230033789,{"$f":"F3753*(1-Elteq!$F$6)","v":25.436865230033789}]
["ANAMET-S",2691703,"70 mm","Fittings for gigant conduit, Straight fixed with flange, IP 54",25,20.801001187014485,{"$f":"F3754*(1-Elteq!$F$6)","v":20.801001187014485}]
["ANAMET-S",2691993,"95 mm","Fittings for gigant conduit, Straight fixed with flange, IP 54",40,25.436865230033789,{"$f":"F3755*(1-Elteq!$F$6)","v":25.436865230033789}]
["ANAMET-S",2692703,"70 mm","Fittings for gigant conduit, 90° elbow fixed with flange, IP 54",40,27.192733574984992,{"$f":"F3756*(1-Elteq!$F$6)","v":27.192733574984992}]
["ANAMET-S",2692993,"95 mm","Fittings for gigant conduit, 90° elbow fixed with flange, IP 54",20,35.414656777534262,{"$f":"F3757*(1-Elteq!$F$6)","v":35.414656777534262}]
["ANAMET-S",2693703,"70 mm","Fittings for gigant conduit, 90° elbow fixed with flange, IP 54",10,27.192733574984992,{"$f":"F3758*(1-Elteq!$F$6)","v":27.192733574984992}]
["ANAMET-S",2693993,"95 mm","Fittings for gigant conduit, 90° elbow fixed with flange, IP 54",20,35.414656777534262,{"$f":"F3759*(1-Elteq!$F$6)","v":35.414656777534262}]
["ANAMET-S",3360060,"6 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",1,17.837392710615369,{"$f":"F3760*(1-Elteq!$F$6)","v":17.837392710615369}]
["ANAMET-S",3360061,"6 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",15,17.837392710615369,{"$f":"F3761*(1-Elteq!$F$6)","v":17.837392710615369}]
["ANAMET-S",3360063,"6 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",30,17.837392710615369,{"$f":"F3762*(1-Elteq!$F$6)","v":17.837392710615369}]
["ANAMET-S",3360100,"10 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",1,18.692101111332356,{"$f":"F3763*(1-Elteq!$F$6)","v":18.692101111332356}]
["ANAMET-S",3360101,"10 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",15,18.692101111332356,{"$f":"F3764*(1-Elteq!$F$6)","v":18.692101111332356}]
["ANAMET-S",3360103,"10 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",30,18.692101111332356,{"$f":"F3765*(1-Elteq!$F$6)","v":18.692101111332356}]
["ANAMET-S",3360131,"13 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",15,21.692870822545252,{"$f":"F3766*(1-Elteq!$F$6)","v":21.692870822545252}]
["ANAMET-S",3360133,"13 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",30,21.692870822545252,{"$f":"F3767*(1-Elteq!$F$6)","v":21.692870822545252}]
["ANAMET-S",3360160,"16 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",1,24.851575781716726,{"$f":"F3768*(1-Elteq!$F$6)","v":24.851575781716726}]
["ANAMET-S",3360161,"16 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",15,24.851575781716726,{"$f":"F3769*(1-Elteq!$F$6)","v":24.851575781716726}]
["ANAMET-S",3360163,"16 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",30,24.851575781716726,{"$f":"F3770*(1-Elteq!$F$6)","v":24.851575781716726}]
["ANAMET-S",3360190,"19 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",1,28.075312901812314,{"$f":"F3771*(1-Elteq!$F$6)","v":28.075312901812314}]
["ANAMET-S",3360191,"19 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",15,28.075312901812314,{"$f":"F3772*(1-Elteq!$F$6)","v":28.075312901812314}]
["ANAMET-S",3360193,"19 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",30,28.075312901812314,{"$f":"F3773*(1-Elteq!$F$6)","v":28.075312901812314}]
["ANAMET-S",3360220,"22 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",1,33.603046580362388,{"$f":"F3774*(1-Elteq!$F$6)","v":33.603046580362388}]
["ANAMET-S",3360221,"22 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",15,33.603046580362388,{"$f":"F3775*(1-Elteq!$F$6)","v":33.603046580362388}]
["ANAMET-S",3360223,"22 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",30,33.603046580362388,{"$f":"F3776*(1-Elteq!$F$6)","v":33.603046580362388}]
["ANAMET-S",3360250,"25 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",1,36.343687647878809,{"$f":"F3777*(1-Elteq!$F$6)","v":36.343687647878809}]
["ANAMET-S",3360251,"25 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",15,36.343687647878809,{"$f":"F3778*(1-Elteq!$F$6)","v":36.343687647878809}]
["ANAMET-S",3360253,"25 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",30,36.343687647878809,{"$f":"F3779*(1-Elteq!$F$6)","v":36.343687647878809}]
["ANAMET-S",3360290,"29 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",1,43.199935471021597,{"$f":"F3780*(1-Elteq!$F$6)","v":43.199935471021597}]
["ANAMET-S",3360291,"29 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",15,43.199935471021597,{"$f":"F3781*(1-Elteq!$F$6)","v":43.199935471021597}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},3360293,"29 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",30,43.199935471021597,{"$f":"F3782*(1-Elteq!$F$6)","v":43.199935471021597}]
["ANAMET-S",3360320,"32 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",1,45.327416164110616,{"$f":"F3783*(1-Elteq!$F$6)","v":45.327416164110616}]
["ANAMET-S",3360321,"32 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",15,45.327416164110616,{"$f":"F3784*(1-Elteq!$F$6)","v":45.327416164110616}]
["ANAMET-S",3360323,"32 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",30,45.327416164110616,{"$f":"F3785*(1-Elteq!$F$6)","v":45.327416164110616}]
["ANAMET-S",3360350,"35 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",1,46.47012413463441,{"$f":"F3786*(1-Elteq!$F$6)","v":46.47012413463441}]
["ANAMET-S",3360351,"35 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",15,46.47012413463441,{"$f":"F3787*(1-Elteq!$F$6)","v":46.47012413463441}]
["ANAMET-S",3360353,"35 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",30,46.47012413463441,{"$f":"F3788*(1-Elteq!$F$6)","v":46.47012413463441}]
["ANAMET-S",3360380,"38 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",1,47.389864696275517,{"$f":"F3789*(1-Elteq!$F$6)","v":47.389864696275517}]
["ANAMET-S",3360381,"38 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",15,47.389864696275517,{"$f":"F3790*(1-Elteq!$F$6)","v":47.389864696275517}]
["ANAMET-S",3360383,"38 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",30,47.389864696275517,{"$f":"F3791*(1-Elteq!$F$6)","v":47.389864696275517}]
["ANAMET-S",3360410,"41 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",1,48.681217606054439,{"$f":"F3792*(1-Elteq!$F$6)","v":48.681217606054439}]
["ANAMET-S",3360411,"41 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",15,48.681217606054439,{"$f":"F3793*(1-Elteq!$F$6)","v":48.681217606054439}]
["ANAMET-S",3360413,"41 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",30,48.681217606054439,{"$f":"F3794*(1-Elteq!$F$6)","v":48.681217606054439}]
["ANAMET-S",3360440,"44 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",1,62.068552447719419,{"$f":"F3795*(1-Elteq!$F$6)","v":62.068552447719419}]
["ANAMET-S",3360441,"44 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",15,62.068552447719419,{"$f":"F3796*(1-Elteq!$F$6)","v":62.068552447719419}]
["ANAMET-S",3360443,"44 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",30,62.068552447719419,{"$f":"F3797*(1-Elteq!$F$6)","v":62.068552447719419}]
["ANAMET-S",3360510,"51 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",1,67.326867173869559,{"$f":"F3798*(1-Elteq!$F$6)","v":67.326867173869559}]
["ANAMET-S",3360511,"51 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",15,67.326867173869559,{"$f":"F3799*(1-Elteq!$F$6)","v":67.326867173869559}]
["ANAMET-S",3360513,"51 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",30,67.326867173869559,{"$f":"F3800*(1-Elteq!$F$6)","v":67.326867173869559}]
["ANAMET-S",3360571,"57 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",15,81.438846094403289,{"$f":"F3801*(1-Elteq!$F$6)","v":81.438846094403289}]
["ANAMET-S",3360573,"57 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",30,81.438846094403289,{"$f":"F3802*(1-Elteq!$F$6)","v":81.438846094403289}]
["ANAMET-S",3360641,"64 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",15,94.891213096992388,{"$f":"F3803*(1-Elteq!$F$6)","v":94.891213096992388}]
["ANAMET-S",3360643,"64 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",30,94.891213096992388,{"$f":"F3804*(1-Elteq!$F$6)","v":94.891213096992388}]
["ANAMET-S",3360701,"70 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",15,135.6292167616009,{"$f":"F3805*(1-Elteq!$F$6)","v":135.6292167616009}]
["ANAMET-S",3360703,"70 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",30,135.6292167616009,{"$f":"F3806*(1-Elteq!$F$6)","v":135.6292167616009}]
["ANAMET-S",3360761,"76 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",15,158.53911802429755,{"$f":"F3807*(1-Elteq!$F$6)","v":158.53911802429755}]
["ANAMET-S",3360763,"76 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",30,158.53911802429755,{"$f":"F3808*(1-Elteq!$F$6)","v":158.53911802429755}]
["ANAMET-S",3360831,"83 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",15,171.14606693487309,{"$f":"F3809*(1-Elteq!$F$6)","v":171.14606693487309}]
["ANAMET-S",3360833,"83 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",30,171.14606693487309,{"$f":"F3810*(1-Elteq!$F$6)","v":171.14606693487309}]
["ANAMET-S",3360891,"89 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",15,175.94915653455439,{"$f":"F3811*(1-Elteq!$F$6)","v":175.94915653455439}]
["ANAMET-S",3360893,"89 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",30,175.94915653455439,{"$f":"F3812*(1-Elteq!$F$6)","v":175.94915653455439}]
["ANAMET-S",3360951,"95 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",15,181.95998626568365,{"$f":"F3813*(1-Elteq!$F$6)","v":181.95998626568365}]
["ANAMET-S",3360953,"95 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",30,181.95998626568365,{"$f":"F3814*(1-Elteq!$F$6)","v":181.95998626568365}]
["ANAMET-S",3361021,"102 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",15,186.62372123481327,{"$f":"F3815*(1-Elteq!$F$6)","v":186.62372123481327}]
["ANAMET-S",3361023,"102 mm","Hiprojacket areo in red, Glassfibre sleeve silicone cover, IP 67",30,186.62372123481327,{"$f":"F3816*(1-Elteq!$F$6)","v":186.62372123481327}]
["ANAMET-S",3469133,"13 mm","Hiprojacket areo in black, Glassfibre sleeve silicone cover, IP 67",30,22.779836940848373,{"$f":"F3817*(1-Elteq!$F$6)","v":22.779836940848373}]
["ANAMET-S",3469163,"16 mm","Hiprojacket areo in black, Glassfibre sleeve silicone cover, IP 67",30,26.096477147978423,{"$f":"F3818*(1-Elteq!$F$6)","v":26.096477147978423}]
["ANAMET-S",3469193,"19 mm","Hiprojacket areo in black, Glassfibre sleeve silicone cover, IP 67",30,29.478149516032584,{"$f":"F3819*(1-Elteq!$F$6)","v":29.478149516032584}]
["ANAMET-S",3469293,"29 mm","Hiprojacket areo in black, Glassfibre sleeve silicone cover, IP 67",30,45.355287090220948,{"$f":"F3820*(1-Elteq!$F$6)","v":45.355287090220948}]
["ANAMET-S",3469353,"35 mm","Hiprojacket areo in black, Glassfibre sleeve silicone cover, IP 67",30,48.792701310495794,{"$f":"F3821*(1-Elteq!$F$6)","v":48.792701310495794}]
["ANAMET-S",3469383,"38 mm","Hiprojacket areo in black, Glassfibre sleeve silicone cover, IP 67",30,49.758893415654121,{"$f":"F3822*(1-Elteq!$F$6)","v":49.758893415654121}]
["ANAMET-S",3469413,"41 mm","Hiprojacket areo in black, Glassfibre sleeve silicone cover, IP 67",30,51.11527848635717,{"$f":"F3823*(1-Elteq!$F$6)","v":51.11527848635717}]
["ANAMET-S",3469511,"51 mm","Hiprojacket areo in black, Glassfibre sleeve silicone cover, IP 67",15,70.689958924516844,{"$f":"F3824*(1-Elteq!$F$6)","v":70.689958924516844}]
["ANAMET-S",3368063,"6 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,14.269914168492294,{"$f":"F3825*(1-Elteq!$F$6)","v":14.269914168492294}]
["ANAMET-S",3368103,"10 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,15.886427882891812,{"$f":"F3826*(1-Elteq!$F$6)","v":15.886427882891812}]
["ANAMET-S",3368133,"13 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,18.441262776339329,{"$f":"F3827*(1-Elteq!$F$6)","v":18.441262776339329}]
["ANAMET-S",3368163,"16 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,21.116871682931631,{"$f":"F3828*(1-Elteq!$F$6)","v":21.116871682931631}]
["ANAMET-S",3368193,"19 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,23.866803059151504,{"$f":"F3829*(1-Elteq!$F$6)","v":23.866803059151504}]
["ANAMET-S",3368223,"22 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,28.567699263094926,{"$f":"F3830*(1-Elteq!$F$6)","v":28.567699263094926}]
["ANAMET-S",3368253,"25 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,30.890276438956299,{"$f":"F3831*(1-Elteq!$F$6)","v":30.890276438956299}]
["ANAMET-S",3368293,"29 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,34.559948376817282,{"$f":"F3832*(1-Elteq!$F$6)","v":34.559948376817282}]
["ANAMET-S",3368323,"32 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,38.526910193188506,{"$f":"F3833*(1-Elteq!$F$6)","v":38.526910193188506}]
["ANAMET-S",3368353,"35 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,39.50239260705029,{"$f":"F3834*(1-Elteq!$F$6)","v":39.50239260705029}]
["ANAMET-S",3368383,"38 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,40.282778538139709,{"$f":"F3835*(1-Elteq!$F$6)","v":40.282778538139709}]
["ANAMET-S",3368413,"41 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,41.388325273849716,{"$f":"F3836*(1-Elteq!$F$6)","v":41.388325273849716}]
["ANAMET-S",3368443,"44 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,52.759663126867018,{"$f":"F3837*(1-Elteq!$F$6)","v":52.759663126867018}]
["ANAMET-S",3368513,"51 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,57.228301613224303,{"$f":"F3838*(1-Elteq!$F$6)","v":57.228301613224303}]
["ANAMET-S",3368573,"57 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,69.222090149372463,{"$f":"F3839*(1-Elteq!$F$6)","v":69.222090149372463}]
["ANAMET-S",3368643,"64 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,75.920402724556666,{"$f":"F3840*(1-Elteq!$F$6)","v":75.920402724556666}]
["ANAMET-S",3368703,"70 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,108.50151534754005,{"$f":"F3841*(1-Elteq!$F$6)","v":108.50151534754005}]
["ANAMET-S",3368763,"76 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,126.82200411073458,{"$f":"F3842*(1-Elteq!$F$6)","v":126.82200411073458}]
["ANAMET-S",3368833,"83 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,136.92056967137984,{"$f":"F3843*(1-Elteq!$F$6)","v":136.92056967137984}]
["ANAMET-S",3368893,"89 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,140.75746716590282,{"$f":"F3844*(1-Elteq!$F$6)","v":140.75746716590282}]
["ANAMET-S",3368953,"95 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,145.56984707428759,{"$f":"F3845*(1-Elteq!$F$6)","v":145.56984707428759}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},3368973,"102 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,149.29526086436925,{"$f":"F3846*(1-Elteq!$F$6)","v":149.29526086436925}]
["ANAMET-S",3368981,"114 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",15,227.54753107349075,{"$f":"F3847*(1-Elteq!$F$6)","v":227.54753107349075}]
["ANAMET-S",3368983,"114 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,227.54753107349075,{"$f":"F3848*(1-Elteq!$F$6)","v":227.54753107349075}]
["ANAMET-S",3368991,"127 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",15,246.54621237203676,{"$f":"F3849*(1-Elteq!$F$6)","v":246.54621237203676}]
["ANAMET-S",3368993,"127 mm","Hiprojacket industrial in red, Glassfibre sleeve silicone cover, IP 67",30,246.54621237203676,{"$f":"F3850*(1-Elteq!$F$6)","v":246.54621237203676}]
["ANAMET-S",3460133,"13 mm","Hiprojacket industrial in grey, Glassfibre sleeve silicone cover, IP 67",30,19.361003337980431,{"$f":"F3851*(1-Elteq!$F$6)","v":19.361003337980431}]
["ANAMET-S",3460163,"16 mm","Hiprojacket industrial in grey, Glassfibre sleeve silicone cover, IP 67",30,22.175966875124416,{"$f":"F3852*(1-Elteq!$F$6)","v":22.175966875124416}]
["ANAMET-S",3460193,"19 mm","Hiprojacket industrial in grey, Glassfibre sleeve silicone cover, IP 67",30,25.055962573192524,{"$f":"F3853*(1-Elteq!$F$6)","v":25.055962573192524}]
["ANAMET-S",3460293,"29 mm","Hiprojacket industrial in grey, Glassfibre sleeve silicone cover, IP 67",30,36.287945795658139,{"$f":"F3854*(1-Elteq!$F$6)","v":36.287945795658139}]
["ANAMET-S",3460353,"35 mm","Hiprojacket industrial in grey, Glassfibre sleeve silicone cover, IP 67",30,41.481228360884174,{"$f":"F3855*(1-Elteq!$F$6)","v":41.481228360884174}]
["ANAMET-S",3460413,"41 mm","Hiprojacket industrial in grey, Glassfibre sleeve silicone cover, IP 67",30,43.460064114718072,{"$f":"F3856*(1-Elteq!$F$6)","v":43.460064114718072}]
["ANAMET-S",3460513,"51 mm","Hiprojacket industrial in grey, Glassfibre sleeve silicone cover, IP 67",30,60.089716693885528,{"$f":"F3857*(1-Elteq!$F$6)","v":60.089716693885528}]
["ANAMET-S",3461133,"13 mm","Hiprojacket industrial in blue, Glassfibre sleeve silicone cover, IP 67",30,19.361003337980431,{"$f":"F3858*(1-Elteq!$F$6)","v":19.361003337980431}]
["ANAMET-S",3461163,"16 mm","Hiprojacket industrial in blue, Glassfibre sleeve silicone cover, IP 67",30,22.175966875124416,{"$f":"F3859*(1-Elteq!$F$6)","v":22.175966875124416}]
["ANAMET-S",3461193,"19 mm","Hiprojacket industrial in blue, Glassfibre sleeve silicone cover, IP 67",30,25.055962573192524,{"$f":"F3860*(1-Elteq!$F$6)","v":25.055962573192524}]
["ANAMET-S",3461293,"29 mm","Hiprojacket industrial in blue, Glassfibre sleeve silicone cover, IP 67",30,36.287945795658139,{"$f":"F3861*(1-Elteq!$F$6)","v":36.287945795658139}]
["ANAMET-S",3461353,"35 mm","Hiprojacket industrial in blue, Glassfibre sleeve silicone cover, IP 67",30,41.481228360884174,{"$f":"F3862*(1-Elteq!$F$6)","v":41.481228360884174}]
["ANAMET-S",3461413,"41 mm","Hiprojacket industrial in blue, Glassfibre sleeve silicone cover, IP 67",30,43.460064114718072,{"$f":"F3863*(1-Elteq!$F$6)","v":43.460064114718072}]
["ANAMET-S",3461513,"51 mm","Hiprojacket industrial in blue, Glassfibre sleeve silicone cover, IP 67",30,60.089716693885528,{"$f":"F3864*(1-Elteq!$F$6)","v":60.089716693885528}]
["ANAMET-S",3462133,"13 mm","Hiprojacket industrial in yellow, Glassfibre sleeve silicone cover, IP 67",30,19.361003337980431,{"$f":"F3865*(1-Elteq!$F$6)","v":19.361003337980431}]
["ANAMET-S",3462163,"16 mm","Hiprojacket industrial in yellow, Glassfibre sleeve silicone cover, IP 67",30,22.175966875124416,{"$f":"F3866*(1-Elteq!$F$6)","v":22.175966875124416}]
["ANAMET-S",3462193,"19 mm","Hiprojacket industrial in yellow, Glassfibre sleeve silicone cover, IP 67",30,25.055962573192524,{"$f":"F3867*(1-Elteq!$F$6)","v":25.055962573192524}]
["ANAMET-S",3462293,"29 mm","Hiprojacket industrial in yellow, Glassfibre sleeve silicone cover, IP 67",30,36.287945795658139,{"$f":"F3868*(1-Elteq!$F$6)","v":36.287945795658139}]
["ANAMET-S",3462353,"35 mm","Hiprojacket industrial in yellow, Glassfibre sleeve silicone cover, IP 67",30,41.481228360884174,{"$f":"F3869*(1-Elteq!$F$6)","v":41.481228360884174}]
["ANAMET-S",3462413,"41 mm","Hiprojacket industrial in yellow, Glassfibre sleeve silicone cover, IP 67",30,43.460064114718072,{"$f":"F3870*(1-Elteq!$F$6)","v":43.460064114718072}]
["ANAMET-S",3462513,"51 mm","Hiprojacket industrial in yellow, Glassfibre sleeve silicone cover, IP 67",30,60.089716693885528,{"$f":"F3871*(1-Elteq!$F$6)","v":60.089716693885528}]
["ANAMET-S",3463133,"13 mm","Hiprojacket industrial in black, Glassfibre sleeve silicone cover, IP 67",30,19.361003337980431,{"$f":"F3872*(1-Elteq!$F$6)","v":19.361003337980431}]
["ANAMET-S",3463163,"16 mm","Hiprojacket industrial in black, Glassfibre sleeve silicone cover, IP 67",30,22.175966875124416,{"$f":"F3873*(1-Elteq!$F$6)","v":22.175966875124416}]
["ANAMET-S",3463193,"19 mm","Hiprojacket industrial in black, Glassfibre sleeve silicone cover, IP 67",30,25.055962573192524,{"$f":"F3874*(1-Elteq!$F$6)","v":25.055962573192524}]
["ANAMET-S",3463293,"29 mm","Hiprojacket industrial in black, Glassfibre sleeve silicone cover, IP 67",30,36.287945795658139,{"$f":"F3875*(1-Elteq!$F$6)","v":36.287945795658139}]
["ANAMET-S",3463353,"35 mm","Hiprojacket industrial in black, Glassfibre sleeve silicone cover, IP 67",30,41.481228360884174,{"$f":"F3876*(1-Elteq!$F$6)","v":41.481228360884174}]
["ANAMET-S",3463383,"38 mm","Hiprojacket industrial in black, Glassfibre sleeve silicone cover, IP 67",30,42.298775526787381,{"$f":"F3877*(1-Elteq!$F$6)","v":42.298775526787381}]
["ANAMET-S",3463413,"41 mm","Hiprojacket industrial in black, Glassfibre sleeve silicone cover, IP 67",30,43.460064114718072,{"$f":"F3878*(1-Elteq!$F$6)","v":43.460064114718072}]
["ANAMET-S",3463513,"51 mm","Hiprojacket industrial in black, Glassfibre sleeve silicone cover, IP 67",30,60.089716693885528,{"$f":"F3879*(1-Elteq!$F$6)","v":60.089716693885528}]
["ANAMET-S",3550045,"HJ-L-02","Hiprojacket light in red, Glassfibre sleeve silicone cover, IP 67",200,1.5421912447719537,{"$f":"F3880*(1-Elteq!$F$6)","v":1.5421912447719537}]
["ANAMET-S",3550065,"HJ-L-04","Hiprojacket light in red, Glassfibre sleeve silicone cover, IP 67",100,2.3690287193786035,{"$f":"F3881*(1-Elteq!$F$6)","v":2.3690287193786035}]
["ANAMET-S",3550085,"HJ-L-05","Hiprojacket light in red, Glassfibre sleeve silicone cover, IP 67",100,3.474575455088619,{"$f":"F3882*(1-Elteq!$F$6)","v":3.474575455088619}]
["ANAMET-S",3550105,"HJ-L-06","Hiprojacket light in red, Glassfibre sleeve silicone cover, IP 67",100,4.3385741645090503,{"$f":"F3883*(1-Elteq!$F$6)","v":4.3385741645090503}]
["ANAMET-S",3550125,"HJ-L-08","Hiprojacket light in red, Glassfibre sleeve silicone cover, IP 67",100,5.2490244174467104,{"$f":"F3884*(1-Elteq!$F$6)","v":5.2490244174467104}]
["ANAMET-S",3550165,"HJ-L-10","Hiprojacket light in red, Glassfibre sleeve silicone cover, IP 67",50,8.4448906114319637,{"$f":"F3885*(1-Elteq!$F$6)","v":8.4448906114319637}]
["ANAMET-S",3550205,"HJ-L-12","Hiprojacket light in red, Glassfibre sleeve silicone cover, IP 67",50,16.174427452698623,{"$f":"F3886*(1-Elteq!$F$6)","v":16.174427452698623}]
["ANAMET-S",8100111,"PG 11","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",10,4.0784455208125756,{"$f":"F3887*(1-Elteq!$F$6)","v":4.0784455208125756}]
["ANAMET-S",8100161,"PG 16","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",10,4.756638056164098,{"$f":"F3888*(1-Elteq!$F$6)","v":4.756638056164098}]
["ANAMET-S",8100211,"PG 21","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",5,6.2988293009360516,{"$f":"F3889*(1-Elteq!$F$6)","v":6.2988293009360516}]
["ANAMET-S",8100291,"PG 29","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",5,10.888241800438133,{"$f":"F3890*(1-Elteq!$F$6)","v":10.888241800438133}]
["ANAMET-S",8100361,"PG 36","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",2,17.846683019318814,{"$f":"F3891*(1-Elteq!$F$6)","v":17.846683019318814}]
["ANAMET-S",8100421,"PG 42","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",2,23.95041583748251,{"$f":"F3892*(1-Elteq!$F$6)","v":23.95041583748251}]
["ANAMET-S",8100481,"PG 48","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",2,36.724590304720074,{"$f":"F3893*(1-Elteq!$F$6)","v":36.724590304720074}]
["ANAMET-S",8120161,"M16 x 1,5","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",10,3.8183168771161027,{"$f":"F3894*(1-Elteq!$F$6)","v":3.8183168771161027}]
["ANAMET-S",8120171,"M20 x 1,5","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",10,4.1063164469229125,{"$f":"F3895*(1-Elteq!$F$6)","v":4.1063164469229125}]
["ANAMET-S",8120201,"M20 x 1,5","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",10,4.1063164469229125,{"$f":"F3896*(1-Elteq!$F$6)","v":4.1063164469229125}]
["ANAMET-S",8120251,"M25 x 1,5","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",5,6.0572812746464679,{"$f":"F3897*(1-Elteq!$F$6)","v":6.0572812746464679}]
["ANAMET-S",8120321,"M32 x 1,5","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",5,9.7455338299143328,{"$f":"F3898*(1-Elteq!$F$6)","v":9.7455338299143328}]
["ANAMET-S",8120401,"M40 x 1,5","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",2,17.846683019318814,{"$f":"F3899*(1-Elteq!$F$6)","v":17.846683019318814}]
["ANAMET-S",8120501,"M50 x 1,5","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",2,23.95041583748251,{"$f":"F3900*(1-Elteq!$F$6)","v":23.95041583748251}]
["ANAMET-S",8120631,"M63 x 1,5","Fittings for Hiprojacket, Straight fixed with male thread, IP 67",2,36.724590304720074,{"$f":"F3901*(1-Elteq!$F$6)","v":36.724590304720074}]
["ANAMET-S",8175120,"13 mm","Fittings for Hiprojacket, Clamping ring for mounting fittings",10,1.6722555666201908,{"$f":"F3902*(1-Elteq!$F$6)","v":1.6722555666201908}]
["ANAMET-S",8175160,"16 mm","Fittings for Hiprojacket, Clamping ring for mounting fittings",10,2.1367710017924657,{"$f":"F3903*(1-Elteq!$F$6)","v":2.1367710017924657}]
["ANAMET-S",8175200,"22 mm","Fittings for Hiprojacket, Clamping ring for mounting fittings",5,2.5548348934475134,{"$f":"F3904*(1-Elteq!$F$6)","v":2.5548348934475134}]
["ANAMET-S",8175260,"25 mm","Fittings for Hiprojacket, Clamping ring for mounting fittings",5,3.3909626767576091,{"$f":"F3905*(1-Elteq!$F$6)","v":3.3909626767576091}]
["ANAMET-S",8175350,"35 mm","Fittings for Hiprojacket, Clamping ring for mounting fittings",2,3.9483811989643396,{"$f":"F3906*(1-Elteq!$F$6)","v":3.9483811989643396}]
["ANAMET-S",8175400,"38 mm","Fittings for Hiprojacket, Clamping ring for mounting fittings",2,6.7819253535152182,{"$f":"F3907*(1-Elteq!$F$6)","v":6.7819253535152182}]
["ANAMET-S",8175500,"51 mm","Fittings for Hiprojacket, Clamping ring for mounting fittings",2,12.449013662616975,{"$f":"F3908*(1-Elteq!$F$6)","v":12.449013662616975}]
["ANAMET-S",3374251,"25 x 0,5 mm","Hiprosiltape in black, Tape from self-fusing rubber",11,5.880765409281004,{"$f":"F3909*(1-Elteq!$F$6)","v":5.880765409281004}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},3374381,"38 x 0,3 mm","Hiprosiltape in black, Tape from self-fusing rubber",11,7.4229566540529577,{"$f":"F3910*(1-Elteq!$F$6)","v":7.4229566540529577}]
["ANAMET-S",3375251,"25 x 0,5 mm","Hiprosiltape in red, Tape from self-fusing rubber",11,5.880765409281004,{"$f":"F3911*(1-Elteq!$F$6)","v":5.880765409281004}]
["ANAMET-S",3375381,"38 x 0,3 mm","Hiprosiltape in red, Tape from self-fusing rubber",11,7.4229566540529577,{"$f":"F3912*(1-Elteq!$F$6)","v":7.4229566540529577}]
["ANAMET-S",3370251,"25 mm","Hiprotape in red, Glassfibre tape with silicone cover",15,15.979330969926268,{"$f":"F3913*(1-Elteq!$F$6)","v":15.979330969926268}]
["ANAMET-S",3370253,"25 mm","Hiprotape in red, Glassfibre tape with silicone cover",30,15.979330969926268,{"$f":"F3914*(1-Elteq!$F$6)","v":15.979330969926268}]
["ANAMET-S",3370501,"51 mm","Hiprotape in red, Glassfibre tape with silicone cover",15,26.375186409081788,{"$f":"F3915*(1-Elteq!$F$6)","v":26.375186409081788}]
["ANAMET-S",3370503,"51 mm","Hiprotape in red, Glassfibre tape with silicone cover",30,26.375186409081788,{"$f":"F3916*(1-Elteq!$F$6)","v":26.375186409081788}]
["ANAMET-S",3370761,"76 mm","Hiprotape in red, Glassfibre tape with silicone cover",15,33.110660219079776,{"$f":"F3917*(1-Elteq!$F$6)","v":33.110660219079776}]
["ANAMET-S",3370763,"76 mm","Hiprotape in red, Glassfibre tape with silicone cover",30,33.110660219079776,{"$f":"F3918*(1-Elteq!$F$6)","v":33.110660219079776}]
["ANAMET-S",3371001,"102 mm","Hiprotape in red, Glassfibre tape with silicone cover",15,43.692321832304209,{"$f":"F3919*(1-Elteq!$F$6)","v":43.692321832304209}]
["ANAMET-S",3371003,"102 mm","Hiprotape in red, Glassfibre tape with silicone cover",30,43.692321832304209,{"$f":"F3920*(1-Elteq!$F$6)","v":43.692321832304209}]
["ANAMET-S",3371271,"127 mm","Hiprotape in red, Glassfibre tape with silicone cover",15,53.707274614618463,{"$f":"F3921*(1-Elteq!$F$6)","v":53.707274614618463}]
["ANAMET-S",3371273,"127 mm","Hiprotape in red, Glassfibre tape with silicone cover",30,53.707274614618463,{"$f":"F3922*(1-Elteq!$F$6)","v":53.707274614618463}]
["ANAMET-S",3376251,"25 mm","Hiprotape Light in grey, Glassfibre tape with silicone cover",15,3.7347040987850924,{"$f":"F3923*(1-Elteq!$F$6)","v":3.7347040987850924}]
["ANAMET-S",3376253,"25 mm","Hiprotape Light in grey, Glassfibre tape with silicone cover",30,3.4002529854610546,{"$f":"F3924*(1-Elteq!$F$6)","v":3.4002529854610546}]
["ANAMET-S",3376501,"51 mm","Hiprotape Light in grey, Glassfibre tape with silicone cover",15,5.5463142959569653,{"$f":"F3925*(1-Elteq!$F$6)","v":5.5463142959569653}]
["ANAMET-S",3376503,"51 mm","Hiprotape Light in grey, Glassfibre tape with silicone cover",30,5.0260570085640177,{"$f":"F3926*(1-Elteq!$F$6)","v":5.0260570085640177}]
["ANAMET-S",3376761,"76 mm","Hiprotape Light in grey, Glassfibre tape with silicone cover",15,7.032763688508247,{"$f":"F3927*(1-Elteq!$F$6)","v":7.032763688508247}]
["ANAMET-S",3376763,"76 mm","Hiprotape Light in grey, Glassfibre tape with silicone cover",30,6.3638614618601705,{"$f":"F3928*(1-Elteq!$F$6)","v":6.3638614618601705}]
["ANAMET-S",3376991,"102 mm","Hiprotape Light in grey, Glassfibre tape with silicone cover",15,8.4170196853216268,{"$f":"F3929*(1-Elteq!$F$6)","v":8.4170196853216268}]
["ANAMET-S",3376993,"102 mm","Hiprotape Light in grey, Glassfibre tape with silicone cover",30,7.6552143716390955,{"$f":"F3930*(1-Elteq!$F$6)","v":7.6552143716390955}]
["ANAMET-S",3365250,"25 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",1,102.58358870344526,{"$f":"F3931*(1-Elteq!$F$6)","v":102.58358870344526}]
["ANAMET-S",3365251,"25 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",15,96.777145763791808,{"$f":"F3932*(1-Elteq!$F$6)","v":96.777145763791808}]
["ANAMET-S",3365256,"25 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",45,96.777145763791808,{"$f":"F3933*(1-Elteq!$F$6)","v":96.777145763791808}]
["ANAMET-S",3365320,"32 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",1,114.19647458275213,{"$f":"F3934*(1-Elteq!$F$6)","v":114.19647458275213}]
["ANAMET-S",3365321,"32 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",15,107.73971003385751,{"$f":"F3935*(1-Elteq!$F$6)","v":107.73971003385751}]
["ANAMET-S",3365326,"32 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",45,107.73971003385751,{"$f":"F3936*(1-Elteq!$F$6)","v":107.73971003385751}]
["ANAMET-S",3365380,"38 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",1,125.44703842262463,{"$f":"F3937*(1-Elteq!$F$6)","v":125.44703842262463}]
["ANAMET-S",3365381,"38 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",15,118.35853288189573,{"$f":"F3938*(1-Elteq!$F$6)","v":118.35853288189573}]
["ANAMET-S",3365386,"38 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",45,118.35853288189573,{"$f":"F3939*(1-Elteq!$F$6)","v":118.35853288189573}]
["ANAMET-S",3365440,"44 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",1,135.33192688309066,{"$f":"F3940*(1-Elteq!$F$6)","v":135.33192688309066}]
["ANAMET-S",3365441,"44 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",15,127.67671251145158,{"$f":"F3941*(1-Elteq!$F$6)","v":127.67671251145158}]
["ANAMET-S",3365446,"44 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",45,127.67671251145158,{"$f":"F3942*(1-Elteq!$F$6)","v":127.67671251145158}]
["ANAMET-S",3365510,"51 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",1,146.59178103166661,{"$f":"F3943*(1-Elteq!$F$6)","v":146.59178103166661}]
["ANAMET-S",3365511,"51 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",15,138.2955353594898,{"$f":"F3944*(1-Elteq!$F$6)","v":138.2955353594898}]
["ANAMET-S",3365516,"51 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",45,138.2955353594898,{"$f":"F3945*(1-Elteq!$F$6)","v":138.2955353594898}]
["ANAMET-S",3365570,"57 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",1,157.86092548894598,{"$f":"F3946*(1-Elteq!$F$6)","v":157.86092548894598}]
["ANAMET-S",3365571,"57 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",15,148.93293882493487,{"$f":"F3947*(1-Elteq!$F$6)","v":148.93293882493487}]
["ANAMET-S",3365576,"57 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",45,148.93293882493487,{"$f":"F3948*(1-Elteq!$F$6)","v":148.93293882493487}]
["ANAMET-S",3365640,"64 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",1,169.39948889862532,{"$f":"F3949*(1-Elteq!$F$6)","v":169.39948889862532}]
["ANAMET-S",3365641,"64 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",15,159.72827753833855,{"$f":"F3950*(1-Elteq!$F$6)","v":159.72827753833855}]
["ANAMET-S",3365646,"64 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",45,159.72827753833855,{"$f":"F3951*(1-Elteq!$F$6)","v":159.72827753833855}]
["ANAMET-S",3365700,"57 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",1,189.11352396733668,{"$f":"F3952*(1-Elteq!$F$6)","v":189.11352396733668}]
["ANAMET-S",3365701,"70 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",15,171.91716255725905,{"$f":"F3953*(1-Elteq!$F$6)","v":171.91716255725905}]
["ANAMET-S",3365706,"70 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",45,171.91716255725905,{"$f":"F3954*(1-Elteq!$F$6)","v":171.91716255725905}]
["ANAMET-S",3365760,"76 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",1,200.56847459868496,{"$f":"F3955*(1-Elteq!$F$6)","v":200.56847459868496}]
["ANAMET-S",3365761,"76 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",15,182.32230830511804,{"$f":"F3956*(1-Elteq!$F$6)","v":182.32230830511804}]
["ANAMET-S",3365766,"76 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",45,182.32230830511804,{"$f":"F3957*(1-Elteq!$F$6)","v":182.32230830511804}]
["ANAMET-S",3365830,"83 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",1,213.22187505277773,{"$f":"F3958*(1-Elteq!$F$6)","v":213.22187505277773}]
["ANAMET-S",3365831,"83 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",15,193.83300078868697,{"$f":"F3959*(1-Elteq!$F$6)","v":193.83300078868697}]
["ANAMET-S",3365836,"83 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",45,193.83300078868697,{"$f":"F3960*(1-Elteq!$F$6)","v":193.83300078868697}]
["ANAMET-S",3365890,"89 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",1,223.38547277434714,{"$f":"F3961*(1-Elteq!$F$6)","v":223.38547277434714}]
["ANAMET-S",3365891,"89 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",15,203.07685794861527,{"$f":"F3962*(1-Elteq!$F$6)","v":203.07685794861527}]
["ANAMET-S",3365896,"89 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",45,203.07685794861527,{"$f":"F3963*(1-Elteq!$F$6)","v":203.07685794861527}]
["ANAMET-S",3365950,"95 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",1,235.14700359290916,{"$f":"F3964*(1-Elteq!$F$6)","v":235.14700359290916}]
["ANAMET-S",3365951,"95 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",15,213.77000326628104,{"$f":"F3965*(1-Elteq!$F$6)","v":213.77000326628104}]
["ANAMET-S",3365956,"95 mm","Hiproblanket Wrap in red, Glassfibre tape with hook and loop",45,213.77000326628104,{"$f":"F3966*(1-Elteq!$F$6)","v":213.77000326628104}]
["ANAMET-S",3369400,"102 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",1,301.1546469308895,{"$f":"F3967*(1-Elteq!$F$6)","v":301.1546469308895}]
["ANAMET-S",3369401,"102 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",15,286.47595917944557,{"$f":"F3968*(1-Elteq!$F$6)","v":286.47595917944557}]
["ANAMET-S",3369406,"102 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",45,286.47595917944557,{"$f":"F3969*(1-Elteq!$F$6)","v":286.47595917944557}]
["ANAMET-S",3369450,"114 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",1,311.93140502688624,{"$f":"F3970*(1-Elteq!$F$6)","v":311.93140502688624}]
["ANAMET-S",3369451,"114 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",15,296.73245998804936,{"$f":"F3971*(1-Elteq!$F$6)","v":296.73245998804936}]
["ANAMET-S",3369456,"114 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",45,296.73245998804936,{"$f":"F3972*(1-Elteq!$F$6)","v":296.73245998804936}]
["ANAMET-S",3369500,"127 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",1,346.84438513443445,{"$f":"F3973*(1-Elteq!$F$6)","v":346.84438513443445}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},3369501,"127 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",15,329.92673298546021,{"$f":"F3974*(1-Elteq!$F$6)","v":329.92673298546021}]
["ANAMET-S",3369506,"127 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",45,329.92673298546021,{"$f":"F3975*(1-Elteq!$F$6)","v":329.92673298546021}]
["ANAMET-S",3369550,"140 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",1,367.37596736904902,{"$f":"F3976*(1-Elteq!$F$6)","v":367.37596736904902}]
["ANAMET-S",3369551,"140 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",15,349.46425218880609,{"$f":"F3977*(1-Elteq!$F$6)","v":349.46425218880609}]
["ANAMET-S",3369556,"140 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",45,349.46425218880609,{"$f":"F3978*(1-Elteq!$F$6)","v":349.46425218880609}]
["ANAMET-S",3369600,"152 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",1,389.61696640509751,{"$f":"F3979*(1-Elteq!$F$6)","v":389.61696640509751}]
["ANAMET-S",3369601,"152 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",15,370.61828510655153,{"$f":"F3980*(1-Elteq!$F$6)","v":370.61828510655153}]
["ANAMET-S",3369606,"152 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",45,370.61828510655153,{"$f":"F3981*(1-Elteq!$F$6)","v":370.61828510655153}]
["ANAMET-S",3369650,"165 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",1,412.71267384186308,{"$f":"F3982*(1-Elteq!$F$6)","v":412.71267384186308}]
["ANAMET-S",3369651,"165 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",15,392.59915549890349,{"$f":"F3983*(1-Elteq!$F$6)","v":392.59915549890349}]
["ANAMET-S",3369656,"165 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",45,392.59915549890349,{"$f":"F3984*(1-Elteq!$F$6)","v":392.59915549890349}]
["ANAMET-S",3369700,"178 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",1,433.94102922923605,{"$f":"F3985*(1-Elteq!$F$6)","v":433.94102922923605}]
["ANAMET-S",3369701,"178 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",15,401.10907827125959,{"$f":"F3986*(1-Elteq!$F$6)","v":401.10907827125959}]
["ANAMET-S",3369706,"178 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",45,401.10907827125959,{"$f":"F3987*(1-Elteq!$F$6)","v":401.10907827125959}]
["ANAMET-S",3369750,"191 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",1,456.69299524397405,{"$f":"F3988*(1-Elteq!$F$6)","v":456.69299524397405}]
["ANAMET-S",3369751,"191 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",15,434.43341559051868,{"$f":"F3989*(1-Elteq!$F$6)","v":434.43341559051868}]
["ANAMET-S",3369756,"191 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",45,434.43341559051868,{"$f":"F3990*(1-Elteq!$F$6)","v":434.43341559051868}]
["ANAMET-S",3369800,"203 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",1,477.40109334395413,{"$f":"F3991*(1-Elteq!$F$6)","v":477.40109334395413}]
["ANAMET-S",3369801,"203 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",15,454.11957973311968,{"$f":"F3992*(1-Elteq!$F$6)","v":454.11957973311968}]
["ANAMET-S",3369806,"203 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",45,454.11957973311968,{"$f":"F3993*(1-Elteq!$F$6)","v":454.11957973311968}]
["ANAMET-S",3369850,"216 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",1,501.01705806811259,{"$f":"F3994*(1-Elteq!$F$6)","v":501.01705806811259}]
["ANAMET-S",3369851,"216 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",15,476.60212679545782,{"$f":"F3995*(1-Elteq!$F$6)","v":476.60212679545782}]
["ANAMET-S",3369856,"216 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",45,476.60212679545782,{"$f":"F3996*(1-Elteq!$F$6)","v":476.60212679545782}]
["ANAMET-S",3369900,"229 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",1,521.70657555068567,{"$f":"F3997*(1-Elteq!$F$6)","v":521.70657555068567}]
["ANAMET-S",3369901,"229 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",15,496.27900062935544,{"$f":"F3998*(1-Elteq!$F$6)","v":496.27900062935544}]
["ANAMET-S",3369906,"229 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",45,496.27900062935544,{"$f":"F3999*(1-Elteq!$F$6)","v":496.27900062935544}]
["ANAMET-S",3369910,"241 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",1,544.81157329615462,{"$f":"F4000*(1-Elteq!$F$6)","v":544.81157329615462}]
["ANAMET-S",3369911,"241 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",15,518.25987102170757,{"$f":"F4001*(1-Elteq!$F$6)","v":518.25987102170757}]
["ANAMET-S",3369916,"241 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",45,518.25987102170757,{"$f":"F4002*(1-Elteq!$F$6)","v":518.25987102170757}]
["ANAMET-S",3369920,"254 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",1,567.06186264090672,{"$f":"F4003*(1-Elteq!$F$6)","v":567.06186264090672}]
["ANAMET-S",3369921,"254 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",15,539.41390393945278,{"$f":"F4004*(1-Elteq!$F$6)","v":539.41390393945278}]
["ANAMET-S",3369926,"254 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",45,539.41390393945278,{"$f":"F4005*(1-Elteq!$F$6)","v":539.41390393945278}]
["ANAMET-S",3369940,"267 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",1,586.73873647480411,{"$f":"F4006*(1-Elteq!$F$6)","v":586.73873647480411}]
["ANAMET-S",3369941,"267 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",15,558.15245659430241,{"$f":"F4007*(1-Elteq!$F$6)","v":558.15245659430241}]
["ANAMET-S",3369946,"267 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",45,558.15245659430241,{"$f":"F4008*(1-Elteq!$F$6)","v":558.15245659430241}]
["ANAMET-S",3369960,"279 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",1,625.23777574188239,{"$f":"F4009*(1-Elteq!$F$6)","v":625.23777574188239}]
["ANAMET-S",3369961,"279 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",15,594.75627288587771,{"$f":"F4010*(1-Elteq!$F$6)","v":594.75627288587771}]
["ANAMET-S",3369966,"279 mm","Hiproblanket Wrap TB in red, Glassfibre tape with hook and loop",45,594.75627288587771,{"$f":"F4011*(1-Elteq!$F$6)","v":594.75627288587771}]
["ANAMET-S",3377250,"25 mm","Hiproblanket Wrap Light in grey, Glassfibre tape with hook and loop",1,22.826288484365605,{"$f":"F4012*(1-Elteq!$F$6)","v":22.826288484365605}]
["ANAMET-S",3377253,"25 mm","Hiproblanket Wrap Light in grey, Glassfibre tape with hook and loop",15,20.763839952200701,{"$f":"F4013*(1-Elteq!$F$6)","v":20.763839952200701}]
["ANAMET-S",3377380,"38 mm","Hiproblanket Wrap Light in grey, Glassfibre tape with hook and loop",1,25.789896960764718,{"$f":"F4014*(1-Elteq!$F$6)","v":25.789896960764718}]
["ANAMET-S",3377383,"38 mm","Hiproblanket Wrap Light in grey, Glassfibre tape with hook and loop",15,23.448739167496448,{"$f":"F4015*(1-Elteq!$F$6)","v":23.448739167496448}]
["ANAMET-S",3377510,"51 mm","Hiproblanket Wrap Light in grey, Glassfibre tape with hook and loop",1,27.657249010157265,{"$f":"F4016*(1-Elteq!$F$6)","v":27.657249010157265}]
["ANAMET-S",3377513,"51 mm","Hiproblanket Wrap Light in grey, Glassfibre tape with hook and loop",15,25.167446277633871,{"$f":"F4017*(1-Elteq!$F$6)","v":25.167446277633871}]
["ANAMET-S",3377640,"64 mm","Hiproblanket Wrap Light in grey, Glassfibre tape with hook and loop",1,30.147051742680663,{"$f":"F4018*(1-Elteq!$F$6)","v":30.147051742680663}]
["ANAMET-S",3377643,"64 mm","Hiproblanket Wrap Light in grey, Glassfibre tape with hook and loop",15,27.369249440350458,{"$f":"F4019*(1-Elteq!$F$6)","v":27.369249440350458}]
["ANAMET-S",3377760,"76 mm","Hiproblanket Wrap Light in grey, Glassfibre tape with hook and loop",1,32.107306879107661,{"$f":"F4020*(1-Elteq!$F$6)","v":32.107306879107661}]
["ANAMET-S",3377763,"76 mm","Hiproblanket Wrap Light in grey, Glassfibre tape with hook and loop",15,29.190149946225773,{"$f":"F4021*(1-Elteq!$F$6)","v":29.190149946225773}]
["ANAMET-S",3377890,"89 mm","Hiproblanket Wrap Light in grey, Glassfibre tape with hook and loop",1,35.070915355506784,{"$f":"F4022*(1-Elteq!$F$6)","v":35.070915355506784}]
["ANAMET-S",3377893,"89 mm","Hiproblanket Wrap Light in grey, Glassfibre tape with hook and loop",15,31.865758852818079,{"$f":"F4023*(1-Elteq!$F$6)","v":31.865758852818079}]
["ANAMET-S",3377990,"102 mm","Hiproblanket Wrap Light in grey, Glassfibre tape with hook and loop",1,42.057227500497802,{"$f":"F4024*(1-Elteq!$F$6)","v":42.057227500497802}]
["ANAMET-S",3377991,"102 mm","Hiproblanket Wrap Light in grey, Glassfibre tape with hook and loop",15,38.22962031467825,{"$f":"F4025*(1-Elteq!$F$6)","v":38.22962031467825}]
["ANAMET-S",3567323,"HBW-MM-20","Hiproblanket Wrap Med in red, Glassfibre tape with hook and loop",15,177.56567024895389,{"$f":"F4026*(1-Elteq!$F$6)","v":177.56567024895389}]
["ANAMET-S",3567383,"HBW-MM-24","Hiproblanket Wrap Med in red, Glassfibre tape with hook and loop",15,184.90501412467586,{"$f":"F4027*(1-Elteq!$F$6)","v":184.90501412467586}]
["ANAMET-S",3567513,"HBW-MM-32","Hiproblanket Wrap Med in red, Glassfibre tape with hook and loop",15,197.40047933081007,{"$f":"F4028*(1-Elteq!$F$6)","v":197.40047933081007}]
["ANAMET-S",3567763,"HBW-MM-48","Hiproblanket Wrap Med in red, Glassfibre tape with hook and loop",15,224.56534197968472,{"$f":"F4029*(1-Elteq!$F$6)","v":224.56534197968472}]
["ANAMET-S",3567993,"HBW-MM-64","Hiproblanket Wrap Med in red, Glassfibre tape with hook and loop",15,250.61536758414587,{"$f":"F4030*(1-Elteq!$F$6)","v":250.61536758414587}]
["ANAMET-S",3366041,"5 mm","Thermojacket S in gold-brown, Heat threated glass fibre",15,5.4162499741087293,{"$f":"F4031*(1-Elteq!$F$6)","v":5.4162499741087293}]
["ANAMET-S",3366043,"5 mm","Thermojacket S in gold-brown, Heat threated glass fibre",30,5.1375407130053636,{"$f":"F4032*(1-Elteq!$F$6)","v":5.1375407130053636}]
["ANAMET-S",3366048,"5 mm","Thermojacket S in gold-brown, Heat threated glass fibre",180,5.1375407130053636,{"$f":"F4033*(1-Elteq!$F$6)","v":5.1375407130053636}]
["ANAMET-S",3366061,"8 mm","Thermojacket S in gold-brown, Heat threated glass fibre",15,8.7143095638318844,{"$f":"F4034*(1-Elteq!$F$6)","v":8.7143095638318844}]
["ANAMET-S",3366063,"8 mm","Thermojacket S in gold-brown, Heat threated glass fibre",30,8.277665054769944,{"$f":"F4035*(1-Elteq!$F$6)","v":8.277665054769944}]
["ANAMET-S",3366068,"8 mm","Thermojacket S in gold-brown, Heat threated glass fibre",120,8.277665054769944,{"$f":"F4036*(1-Elteq!$F$6)","v":8.277665054769944}]
["ANAMET-S",3366101,"12 mm","Thermojacket S in gold-brown, Heat threated glass fibre",15,18.840746050587484,{"$f":"F4037*(1-Elteq!$F$6)","v":18.840746050587484}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},3366103,"12 mm","Thermojacket S in gold-brown, Heat threated glass fibre",30,17.902424871539484,{"$f":"F4038*(1-Elteq!$F$6)","v":17.902424871539484}]
["ANAMET-S",3366108,"12 mm","Thermojacket S in gold-brown, Heat threated glass fibre",75,17.902424871539484,{"$f":"F4039*(1-Elteq!$F$6)","v":17.902424871539484}]
["ANAMET-S",3366141,"20 mm","Thermojacket S in gold-brown, Heat threated glass fibre",15,24.972349794861511,{"$f":"F4040*(1-Elteq!$F$6)","v":24.972349794861511}]
["ANAMET-S",3366143,"20 mm","Thermojacket S in gold-brown, Heat threated glass fibre",30,23.718158119896373,{"$f":"F4041*(1-Elteq!$F$6)","v":23.718158119896373}]
["ANAMET-S",3366148,"20 mm","Thermojacket S in gold-brown, Heat threated glass fibre",60,23.718158119896373,{"$f":"F4042*(1-Elteq!$F$6)","v":23.718158119896373}]
["ANAMET-S",3366221,"30 mm","Thermojacket S in gold-brown, Heat threated glass fibre",15,37.235557283409577,{"$f":"F4043*(1-Elteq!$F$6)","v":37.235557283409577}]
["ANAMET-S",3366223,"30 mm","Thermojacket S in gold-brown, Heat threated glass fibre",30,35.368205234017033,{"$f":"F4044*(1-Elteq!$F$6)","v":35.368205234017033}]
["ANAMET-S",3366228,"30 mm","Thermojacket S in gold-brown, Heat threated glass fibre",45,35.368205234017033,{"$f":"F4045*(1-Elteq!$F$6)","v":35.368205234017033}]
["ANAMET-S",3366441,"50 mm","Thermojacket S in gold-brown, Heat threated glass fibre",15,57.497720565624228,{"$f":"F4046*(1-Elteq!$F$6)","v":57.497720565624228}]
["ANAMET-S",3366443,"50 mm","Thermojacket S in gold-brown, Heat threated glass fibre",30,54.627015176259562,{"$f":"F4047*(1-Elteq!$F$6)","v":54.627015176259562}]
["ANAMET-S",8100111,"PG 11","Fittings for Thermojacket S, Clamping ring for mounting fittings",10,4.0784455208125756,{"$f":"F4048*(1-Elteq!$F$6)","v":4.0784455208125756}]
["ANAMET-S",8100161,"PG 16","Fittings for Thermojacket S, Clamping ring for mounting fittings",10,4.756638056164098,{"$f":"F4049*(1-Elteq!$F$6)","v":4.756638056164098}]
["ANAMET-S",8100211,"PG 21","Fittings for Thermojacket S, Clamping ring for mounting fittings",5,6.2988293009360516,{"$f":"F4050*(1-Elteq!$F$6)","v":6.2988293009360516}]
["ANAMET-S",8100291,"PG 29","Fittings for Thermojacket S, Clamping ring for mounting fittings",5,10.888241800438133,{"$f":"F4051*(1-Elteq!$F$6)","v":10.888241800438133}]
["ANAMET-S",8100361,"PG 36","Fittings for Thermojacket S, Clamping ring for mounting fittings",2,17.846683019318814,{"$f":"F4052*(1-Elteq!$F$6)","v":17.846683019318814}]
["ANAMET-S",8100421,"PG 42","Fittings for Thermojacket S, Clamping ring for mounting fittings",2,23.95041583748251,{"$f":"F4053*(1-Elteq!$F$6)","v":23.95041583748251}]
["ANAMET-S",8100481,"PG 48","Fittings for Thermojacket S, Clamping ring for mounting fittings",2,36.724590304720074,{"$f":"F4054*(1-Elteq!$F$6)","v":36.724590304720074}]
["ANAMET-S",8120161,"M16 x 1,5","Fittings for Thermojacket S, Clamping ring for mounting fittings",10,3.8183168771161027,{"$f":"F4055*(1-Elteq!$F$6)","v":3.8183168771161027}]
["ANAMET-S",8120171,"M20 x 1,5","Fittings for Thermojacket S, Clamping ring for mounting fittings",10,4.1063164469229125,{"$f":"F4056*(1-Elteq!$F$6)","v":4.1063164469229125}]
["ANAMET-S",8120201,"M20 x 1,5","Fittings for Thermojacket S, Clamping ring for mounting fittings",10,4.1063164469229125,{"$f":"F4057*(1-Elteq!$F$6)","v":4.1063164469229125}]
["ANAMET-S",8120251,"M25 x 1,5","Fittings for Thermojacket S, Clamping ring for mounting fittings",5,6.0572812746464679,{"$f":"F4058*(1-Elteq!$F$6)","v":6.0572812746464679}]
["ANAMET-S",8120321,"M32 x 1,5","Fittings for Thermojacket S, Clamping ring for mounting fittings",5,9.7455338299143328,{"$f":"F4059*(1-Elteq!$F$6)","v":9.7455338299143328}]
["ANAMET-S",8120401,"M40 x 1,5","Fittings for Thermojacket S, Clamping ring for mounting fittings",2,17.846683019318814,{"$f":"F4060*(1-Elteq!$F$6)","v":17.846683019318814}]
["ANAMET-S",8120501,"M50 x 1,5","Fittings for Thermojacket S, Clamping ring for mounting fittings",2,23.95041583748251,{"$f":"F4061*(1-Elteq!$F$6)","v":23.95041583748251}]
["ANAMET-S",8120631,"M63 x 1,5","Fittings for Thermojacket S, Clamping ring for mounting fittings",2,36.724590304720074,{"$f":"F4062*(1-Elteq!$F$6)","v":36.724590304720074}]
["ANAMET-S",8176120,"TJ- 10","Fittings for Thermojacket S, Clamping ring for mounting fittings",10,1.6722555666201908,{"$f":"F4063*(1-Elteq!$F$6)","v":1.6722555666201908}]
["ANAMET-S",8176160,"TJ- 10","Fittings for Thermojacket S, Clamping ring for mounting fittings",10,2.1367710017924657,{"$f":"F4064*(1-Elteq!$F$6)","v":2.1367710017924657}]
["ANAMET-S",8176200,"TJ- 14","Fittings for Thermojacket S, Clamping ring for mounting fittings",5,2.5548348934475134,{"$f":"F4065*(1-Elteq!$F$6)","v":2.5548348934475134}]
["ANAMET-S",8176260,"TJ- 14","Fittings for Thermojacket S, Clamping ring for mounting fittings",5,3.3909626767576091,{"$f":"F4066*(1-Elteq!$F$6)","v":3.3909626767576091}]
["ANAMET-S",8176350,"TJ- 22","Fittings for Thermojacket S, Clamping ring for mounting fittings",2,3.9483811989643396,{"$f":"F4067*(1-Elteq!$F$6)","v":3.9483811989643396}]
["ANAMET-S",8176400,"TJ- 22","Fittings for Thermojacket S, Clamping ring for mounting fittings",2,6.7819253535152182,{"$f":"F4068*(1-Elteq!$F$6)","v":6.7819253535152182}]
["ANAMET-S",8176500,"TJ- 44","Fittings for Thermojacket S, Clamping ring for mounting fittings",2,12.449013662616975,{"$f":"F4069*(1-Elteq!$F$6)","v":12.449013662616975}]
["ANAMET-S",3470161,"24 - 50 mm","Silicajacket in white, Sleeve from silica fibres",15,90.664122636924688,{"$f":"F4070*(1-Elteq!$F$6)","v":90.664122636924688}]
["ANAMET-S",3470241,"36 - 60 mm","Silicajacket in white, Sleeve from silica fibres",15,125.25194193985229,{"$f":"F4071*(1-Elteq!$F$6)","v":125.25194193985229}]
["ANAMET-S",3470321,"49 - 70 mm","Silicajacket in white, Sleeve from silica fibres",15,148.50558462457639,{"$f":"F4072*(1-Elteq!$F$6)","v":148.50558462457639}]
["ANAMET-S",3470481,"74 - 140 mm","Silicajacket in white, Sleeve from silica fibres",15,194.72487042421776,{"$f":"F4073*(1-Elteq!$F$6)","v":194.72487042421776}]
["ANAMET-S",3470641,"100 - 200 mm","Silicajacket in white, Sleeve from silica fibres",15,214.1044543796051,{"$f":"F4074*(1-Elteq!$F$6)","v":214.1044543796051}]
["ANAMET-S",3571028,"TJ-L-02","Thermojacket Light in white, Heat threated glass fibre",500,0.4273542003584932,{"$f":"F4075*(1-Elteq!$F$6)","v":0.4273542003584932}]
["ANAMET-S",3571048,"TJ-L-04","Thermojacket Light in white, Heat threated glass fibre",300,0.70606346146185839,{"$f":"F4076*(1-Elteq!$F$6)","v":0.70606346146185839}]
["ANAMET-S",3571058,"TJ-L-05","Thermojacket Light in white, Heat threated glass fibre",300,0.90115994423421386,{"$f":"F4077*(1-Elteq!$F$6)","v":0.90115994423421386}]
["ANAMET-S",3571068,"TJ-L-06","Thermojacket Light in white, Heat threated glass fibre",300,1.0776758095996783,{"$f":"F4078*(1-Elteq!$F$6)","v":1.0776758095996783}]
["ANAMET-S",3571088,"TJ-L-08","Thermojacket Light in white, Heat threated glass fibre",200,1.2913529097789249,{"$f":"F4079*(1-Elteq!$F$6)","v":1.2913529097789249}]
["ANAMET-S",3571108,"TJ-L-10","Thermojacket Light in white, Heat threated glass fibre",200,2.2668353236407031,{"$f":"F4080*(1-Elteq!$F$6)","v":2.2668353236407031}]
["ANAMET-S",3571128,"TJ-L-12","Thermojacket Light in white, Heat threated glass fibre",100,3.0658018721370164,{"$f":"F4081*(1-Elteq!$F$6)","v":3.0658018721370164}]
["ANAMET-S",3571168,"TJ-L-16","Thermojacket Light in white, Heat threated glass fibre",100,4.0970261382194675,{"$f":"F4082*(1-Elteq!$F$6)","v":4.0970261382194675}]
["ANAMET-S",3571188,"TJ-L-18","Thermojacket Light in white, Heat threated glass fibre",100,5.1747019478191456,{"$f":"F4083*(1-Elteq!$F$6)","v":5.1747019478191456}]
["ANAMET-S",3571228,"TJ-L-22","Thermojacket Light in white, Heat threated glass fibre",50,6.6797319577773182,{"$f":"F4084*(1-Elteq!$F$6)","v":6.6797319577773182}]
["ANAMET-S",3363400,"1,0 X 1 meter","Hiproblanket medium in red, Glassfibre blanket with silicone cover",1,208.47452730531714,{"$f":"F4085*(1-Elteq!$F$6)","v":208.47452730531714}]
["ANAMET-S",3363401,"1,0 X 25 meter","Hiproblanket medium in red, Glassfibre blanket with silicone cover",25,173.72877275443091,{"$f":"F4086*(1-Elteq!$F$6)","v":173.72877275443091}]
["ANAMET-S",3363405,"1,0 X 50 meter","Hiproblanket medium in red, Glassfibre blanket with silicone cover",50,173.72877275443091,{"$f":"F4087*(1-Elteq!$F$6)","v":173.72877275443091}]
["ANAMET-S",3364400,"1,016 X 1 meter","Hiproblanket heavy in red, Glassfibre blanket with silicone cover",1,607.37251210515672,{"$f":"F4088*(1-Elteq!$F$6)","v":607.37251210515672}]
["ANAMET-S",3364401,"1,016 X 45 meter","Hiproblanket heavy in red, Glassfibre blanket with silicone cover",15,506.13601816371101,{"$f":"F4089*(1-Elteq!$F$6)","v":506.13601816371101}]
["ANAMET-S",3364405,"1,016 X 45 meter","Hiproblanket heavy in red, Glassfibre blanket with silicone cover",45,506.13601816371101,{"$f":"F4090*(1-Elteq!$F$6)","v":506.13601816371101}]
["ANAMET-S",3363500,"1,0 X 25 meter","Hiproblanket medium in red, Glassfibre blanket with silicone cover",1,306.58018721370166,{"$f":"F4091*(1-Elteq!$F$6)","v":306.58018721370166}]
["ANAMET-S",3363501,"1,0 X 25 meter","Hiproblanket medium in red, Glassfibre blanket with silicone cover",25,250.83833499302861,{"$f":"F4092*(1-Elteq!$F$6)","v":250.83833499302861}]
["ANAMET-S",3363505,"1,0 X 50 meter","Hiproblanket medium in red, Glassfibre blanket with silicone cover",50,250.83833499302861,{"$f":"F4093*(1-Elteq!$F$6)","v":250.83833499302861}]
["ANAMET-S",3364700,"1,000 X 50 meter","Hiproblanket medium in silver, Glassfibre blanket with alumium sheet",1,90.060252571200721,{"$f":"F4094*(1-Elteq!$F$6)","v":90.060252571200721}]
["ANAMET-S",3364701,"1,000 X 50 meter","Hiproblanket medium in silver, Glassfibre blanket with alumium sheet",25,75.047113706432782,{"$f":"F4095*(1-Elteq!$F$6)","v":75.047113706432782}]
["ANAMET-S",3364703,"1,000 X 50 meter","Hiproblanket medium in silver, Glassfibre blanket with alumium sheet",50,75.047113706432782,{"$f":"F4096*(1-Elteq!$F$6)","v":75.047113706432782}]
["ANAMET-S",3364200,"1,524 X 1 meter","Hiproblanket light in grey, Glassfibre blanket with silicone cover",1,143.53526946823303,{"$f":"F4097*(1-Elteq!$F$6)","v":143.53526946823303}]
["ANAMET-S",3364201,"1,524 X 15 meter","Hiproblanket light in grey, Glassfibre blanket with silicone cover",15,124.8060071220869,{"$f":"F4098*(1-Elteq!$F$6)","v":124.8060071220869}]
["ANAMET-S",3364205,"1,524 X 45 meter","Hiproblanket light in grey, Glassfibre blanket with silicone cover",45,124.8060071220869,{"$f":"F4099*(1-Elteq!$F$6)","v":124.8060071220869}]
["ANAMET-S",3474200,"0,95 x 1 meter","Silicablanket in white, Blanket from silica fibres",1,108.69661183031239,{"$f":"F4100*(1-Elteq!$F$6)","v":108.69661183031239}]
["ANAMET-S",3474205,"0,95 x 1 meter","Silicablanket in white, Blanket from silica fibres",45,90.580509858593658,{"$f":"F4101*(1-Elteq!$F$6)","v":90.580509858593658}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"ANAMET-S"},3474300,"0,920 x 1 meter","Silicablanket in white, Blanket from silica fibres",1,62.988293009360511,{"$f":"F4102*(1-Elteq!$F$6)","v":62.988293009360511}]
["ANAMET-S",3474305,"0,920 x 1 meter","Silicablanket in white, Blanket from silica fibres",45,52.490244174467094,{"$f":"F4103*(1-Elteq!$F$6)","v":52.490244174467094}]

{"sheet":"BIMED","index":4,"n_rows":418,"n_cols":8,"rows_kept":418,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["sheetname","Názov tovaru","Typ a veľkosť závitu","Popis","Balenie","Cena za ks","Cena za kus po zľave","EAN"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"BIMED"},"BS-01","Pg   7","Vývodka šedá Pg7",100,0.1517,{"$f":"F5*(1-Elteq!$F$7)","v":0.1517},869760630586]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"BIMED"},"BS-02","Pg   9","Vývodka šedá Pg9",50,0.16200000000000001,{"$f":"F6*(1-Elteq!$F$7)","v":0.16200000000000001},869760630594]
["BIMED","BS-03","Pg 11","Vývodka šedá Pg11",50,0.16739999999999999,{"$f":"F7*(1-Elteq!$F$7)","v":0.16739999999999999},869760630603]
["BIMED","BS-04","Pg 13.5","Vývodka šedá Pg13,5",50,0.19639999999999999,{"$f":"F8*(1-Elteq!$F$7)","v":0.19639999999999999},869760630612]
["BIMED","BS-05","Pg 16","Vývodka šedá Pg16",50,0.24260000000000001,{"$f":"F9*(1-Elteq!$F$7)","v":0.24260000000000001},869760630621]
["BIMED","BS-06","Pg 21","Vývodka šedá Pg21",25,0.37130000000000002,{"$f":"F10*(1-Elteq!$F$7)","v":0.37130000000000002},869760630630]
["BIMED","BS-07","Pg 29","Vývodka šedá Pg29",20,0.8024,{"$f":"F11*(1-Elteq!$F$7)","v":0.8024},869760630638]
["BIMED","BS-08","Pg 36","Vývodka šedá Pg36",10,1.5626,{"$f":"F12*(1-Elteq!$F$7)","v":1.5626},869760630647]
["BIMED","BS-09","Pg 42","Vývodka šedá Pg42","1 (10)",2.4689000000000001,{"$f":"F13*(1-Elteq!$F$7)","v":2.4689000000000001},869760630655]
["BIMED","BS-10","Pg 48","Vývodka šedá Pg48","1 (10)",2.4108000000000001,{"$f":"F14*(1-Elteq!$F$7)","v":2.4108000000000001},869760630662]
["BIMED","BS-11","Pg   7","Vývodka svetlo šedá Pg7",100,0.1517,{"$f":"F15*(1-Elteq!$F$7)","v":0.1517},869760630670]
["BIMED","BS-12","Pg   9","Vývodka svetlo šedá Pg9",50,0.16200000000000001,{"$f":"F16*(1-Elteq!$F$7)","v":0.16200000000000001},869760630683]
["BIMED","BS-13","Pg 11","Vývodka svetlo šedá Pg11",50,0.16739999999999999,{"$f":"F17*(1-Elteq!$F$7)","v":0.16739999999999999},869760630696]
["BIMED","BS-14","Pg 13.5","Vývodka svetlo šedá Pg13,5",50,0.19639999999999999,{"$f":"F18*(1-Elteq!$F$7)","v":0.19639999999999999},869760630708]
["BIMED","BS-15","Pg 16","Vývodka svetlo šedá Pg16",50,0.24260000000000001,{"$f":"F19*(1-Elteq!$F$7)","v":0.24260000000000001},869760630722]
["BIMED","BS-16","Pg 21","Vývodka svetlo šedá Pg21",25,0.37130000000000002,{"$f":"F20*(1-Elteq!$F$7)","v":0.37130000000000002},869760630735]
["BIMED","BS-17","Pg 29","Vývodka svetlo šedá Pg29",20,0.8024,{"$f":"F21*(1-Elteq!$F$7)","v":0.8024},869760630747]
["BIMED","BS-18","Pg 36","Vývodka svetlo šedá Pg36",10,1.5626,{"$f":"F22*(1-Elteq!$F$7)","v":1.5626},869760630758]
["BIMED","BS-19","Pg 42","Vývodka svetlo šedá Pg42","1 (10)",2.4689000000000001,{"$f":"F23*(1-Elteq!$F$7)","v":2.4689000000000001},869760630770]
["BIMED","BS-20","Pg 48","Vývodka svetlo šedá Pg48","1 (10)",2.4108000000000001,{"$f":"F24*(1-Elteq!$F$7)","v":2.4108000000000001},869760630781]
["BIMED","BS-21","Pg   7","Vývodka čierna Pg7",100,0.1517,{"$f":"F25*(1-Elteq!$F$7)","v":0.1517},869760630790]
["BIMED","BS-22","Pg   9","Vývodka čierna Pg9",50,0.16200000000000001,{"$f":"F26*(1-Elteq!$F$7)","v":0.16200000000000001},869760630799]
["BIMED","BS-23","Pg 11","Vývodka čierna Pg11",50,0.16739999999999999,{"$f":"F27*(1-Elteq!$F$7)","v":0.16739999999999999},869760630808]
["BIMED","BS-24","Pg 13.5","Vývodka čiernaPg13,5",50,0.19639999999999999,{"$f":"F28*(1-Elteq!$F$7)","v":0.19639999999999999},869760630816]
["BIMED","BS-25","Pg 16","Vývodka čierna Pg16",50,0.24260000000000001,{"$f":"F29*(1-Elteq!$F$7)","v":0.24260000000000001},869760630827]
["BIMED","BS-26","Pg 21","Vývodka čierna Pg21",25,0.37130000000000002,{"$f":"F30*(1-Elteq!$F$7)","v":0.37130000000000002},869760630835]
["BIMED","BS-27","Pg 29","Vývodka čierna Pg29",20,0.8024,{"$f":"F31*(1-Elteq!$F$7)","v":0.8024},869760630843]
["BIMED","BS-28","Pg 36","Vývodka čierna Pg36",10,1.5626,{"$f":"F32*(1-Elteq!$F$7)","v":1.5626},869760630850]
["BIMED","BS-29","Pg 42","Vývodka čierna Pg42","1 (10)",2.4689000000000001,{"$f":"F33*(1-Elteq!$F$7)","v":2.4689000000000001},869760630856]
["BIMED","BS-30","Pg 48","Vývodka čierna Pg48","1 (10)",2.4108000000000001,{"$f":"F34*(1-Elteq!$F$7)","v":2.4108000000000001},869760630860]
["BIMED","BD-11","PG  7","Vývodka Pq 7 svetlošedá",100,0.1074,{"$f":"F35*(1-Elteq!$F$7)","v":0.1074},869760631223]
["BIMED","BD-12","PG  9","Vývodka Pq 9 svetlošedá",50,0.11509999999999999,{"$f":"F36*(1-Elteq!$F$7)","v":0.11509999999999999},869760631224]
["BIMED","BD-13","Pg 11","Vývodka Pq 11 svetlošedá",50,0.1232,{"$f":"F37*(1-Elteq!$F$7)","v":0.1232},869760631226]
["BIMED","BD-14","PG 13,5","Vývodka Pq 13,5 svetlošedá",50,0.1457,{"$f":"F38*(1-Elteq!$F$7)","v":0.1457},869760631228]
["BIMED","BD-15","PG 16","Vývodka Pq 16 svetlošedá",50,0.15690000000000001,{"$f":"F39*(1-Elteq!$F$7)","v":0.15690000000000001},869760631229]
["BIMED","BD-16","PG 21","Vývodka Pq 21 svetlošedá",25,0.22420000000000001,{"$f":"F40*(1-Elteq!$F$7)","v":0.22420000000000001},869760631231]
["BIMED","BD-17","PG 29","Vývodka Pq 29 svetlošedá",20,0.36430000000000001,{"$f":"F41*(1-Elteq!$F$7)","v":0.36430000000000001},869760631232]
["BIMED","BD-18","PG 36","Vývodka Pq 36 svetlošedá",10,0.72829999999999995,{"$f":"F42*(1-Elteq!$F$7)","v":0.72829999999999995},869760631234]
["BIMED","BL-01","Pg   7","Matica Pq 7 šedá",100,3.1600000000000003E-2,{"$f":"F43*(1-Elteq!$F$7)","v":3.1600000000000003E-2},869760631280]
["BIMED","BL-02","Pg   9","Matica Pq 9 šedá",50,3.1600000000000003E-2,{"$f":"F44*(1-Elteq!$F$7)","v":3.1600000000000003E-2},869760631282]
["BIMED","BL-03","Pg 11","Matica Pq 11 šedá",50,3.4799999999999998E-2,{"$f":"F45*(1-Elteq!$F$7)","v":3.4799999999999998E-2},869760631284]
["BIMED","BL-04","Pg 13.5","Matica Pq 13,5 šedá",50,3.7699999999999997E-2,{"$f":"F46*(1-Elteq!$F$7)","v":3.7699999999999997E-2},869760631285]
["BIMED","BL-05","Pg 16","Matica Pq 16 šedá",50,4.2099999999999999E-2,{"$f":"F47*(1-Elteq!$F$7)","v":4.2099999999999999E-2},869760631286]
["BIMED","BL-06","Pg 21","Matica Pq 21 šedá",25,5.8700000000000002E-2,{"$f":"F48*(1-Elteq!$F$7)","v":5.8700000000000002E-2},869760631288]
["BIMED","BL-07","Pg 29","Matica Pq 29 šedá",20,0.1021,{"$f":"F49*(1-Elteq!$F$7)","v":0.1021},869760631289]
["BIMED","BL-08","Pg 36","Matica Pq 36 šedá",10,0.17050000000000001,{"$f":"F50*(1-Elteq!$F$7)","v":0.17050000000000001},869760631290]
["BIMED","BL-09","Pg 42","Matica Pq 42 šedá","1 (10)",0.33639999999999998,{"$f":"F51*(1-Elteq!$F$7)","v":0.33639999999999998},869760631293]
["BIMED","BL-10","Pg 48","Matica Pq 48 šedá","1 (10)",0.50409999999999999,{"$f":"F52*(1-Elteq!$F$7)","v":0.50409999999999999},869760631294]
["BIMED","BL-11","Pg   7","Matica Pq 7 svetlo šedá",100,3.1600000000000003E-2,{"$f":"F53*(1-Elteq!$F$7)","v":3.1600000000000003E-2},869760631295]
["BIMED","BL-12","Pg   9","Matica Pq 9 svetlo šedá",50,3.1600000000000003E-2,{"$f":"F54*(1-Elteq!$F$7)","v":3.1600000000000003E-2},869760631296]
["BIMED","BL-13","Pg 11","Matica Pq 11 svetlo šedá",50,3.4799999999999998E-2,{"$f":"F55*(1-Elteq!$F$7)","v":3.4799999999999998E-2},869760631297]
["BIMED","BL-14","Pg 13.5","Matica Pq 13,5 svetlo šedá",50,3.7699999999999997E-2,{"$f":"F56*(1-Elteq!$F$7)","v":3.7699999999999997E-2},869760631298]
["BIMED","BL-15","Pg 16","Matica Pq 16 svetlo šedá",50,4.2099999999999999E-2,{"$f":"F57*(1-Elteq!$F$7)","v":4.2099999999999999E-2},869760631299]
["BIMED","BL-16","Pg 21","Matica Pq 21 svetlo šedá",25,5.8700000000000002E-2,{"$f":"F58*(1-Elteq!$F$7)","v":5.8700000000000002E-2},869760631300]
["BIMED","BL-17","Pg 29","Matica Pq 29 svetlo šedá",20,0.1021,{"$f":"F59*(1-Elteq!$F$7)","v":0.1021},869760631301]
["BIMED","BL-18","Pg 36","Matica Pq 36 svetlo šedá",10,0.17050000000000001,{"$f":"F60*(1-Elteq!$F$7)","v":0.17050000000000001},869760631302]
["BIMED","BL-19","Pg 42","Matica Pq 42 svetlo šedá","1 (10)",0.33639999999999998,{"$f":"F61*(1-Elteq!$F$7)","v":0.33639999999999998},869760631303]
["BIMED","BL-20","Pg 48","Matica Pq 48 svetlo šedá","1 (10)",0.50409999999999999,{"$f":"F62*(1-Elteq!$F$7)","v":0.50409999999999999},869760631304]
["BIMED","BL-21","Pg   7","Matica Pq 7 čierna",100,3.1600000000000003E-2,{"$f":"F63*(1-Elteq!$F$7)","v":3.1600000000000003E-2},869760631305]
["BIMED","BL-22","Pg   9","Matica Pq 9 čierna",50,3.1600000000000003E-2,{"$f":"F64*(1-Elteq!$F$7)","v":3.1600000000000003E-2},869760631306]
["BIMED","BL-23","Pg 11","Matica Pq 11 čierna",50,3.4799999999999998E-2,{"$f":"F65*(1-Elteq!$F$7)","v":3.4799999999999998E-2},869760631307]
["BIMED","BL-24","Pg 13.5","Matica Pq 13,5 čierna",50,3.7699999999999997E-2,{"$f":"F66*(1-Elteq!$F$7)","v":3.7699999999999997E-2},869760631308]
["BIMED","BL-25","Pg 16","Matica Pq 16 čierna",50,4.2099999999999999E-2,{"$f":"F67*(1-Elteq!$F$7)","v":4.2099999999999999E-2},869760631309]
["BIMED","BL-26","Pg 21","Matica Pq 21 čierna",25,5.8700000000000002E-2,{"$f":"F68*(1-Elteq!$F$7)","v":5.8700000000000002E-2},869760631310]
["BIMED","BL-27","Pg 29","Matica Pq 29 čierna",20,0.1021,{"$f":"F69*(1-Elteq!$F$7)","v":0.1021},869760631311]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"BIMED"},"BL-28","Pg 36","Matica Pq 36 čierna",10,0.17050000000000001,{"$f":"F70*(1-Elteq!$F$7)","v":0.17050000000000001},869760631312]
["BIMED","BL-29","Pg 42","Matica Pq 42 čierna","1 (10)",0.33639999999999998,{"$f":"F71*(1-Elteq!$F$7)","v":0.33639999999999998},869760631313]
["BIMED","BL-30","Pg 48","Matica Pq 48 čierna","1 (10)",0.50409999999999999,{"$f":"F72*(1-Elteq!$F$7)","v":0.50409999999999999},869760631314]
["BIMED","BMBS-1S","M12","Záslepka s metrickým závitom M12x1,5 svetlošedá",100,8.77E-2,{"$f":"F73*(1-Elteq!$F$7)","v":8.77E-2}]
["BIMED","BMBS-11","M16","Záslepka s metrickým závitom M16x1,5 svetlošedá",50,9.3100000000000002E-2,{"$f":"F74*(1-Elteq!$F$7)","v":9.3100000000000002E-2},869760632230]
["BIMED","BMBS-12","M20","Záslepka s metrickým závitom M20x1,5 svetlošedá",50,0.1096,{"$f":"F75*(1-Elteq!$F$7)","v":0.1096}]
["BIMED","BMBS-13","M25","Záslepka s metrickým závitom M25x1,5 svetlošedá",25,0.1205,{"$f":"F76*(1-Elteq!$F$7)","v":0.1205}]
["BIMED","BMBS-14","M32","Záslepka s metrickým závitom M32x1,5 svetlošedá",20,0.2082,{"$f":"F77*(1-Elteq!$F$7)","v":0.2082}]
["BIMED","BMBS-15","M40","Záslepka s metrickým závitom M40x1,5 svetlošedá",10,0.54790000000000005,{"$f":"F78*(1-Elteq!$F$7)","v":0.54790000000000005}]
["BIMED","BMBS-16","M50","Záslepka s metrickým závitom M50x1,5 svetlošedá",10,0.92288180250000029,{"$f":"F79*(1-Elteq!$F$7)","v":0.92288180250000029}]
["BIMED","BMBS-2S","M12","Záslepka s metrickým závitom M12x1,5 čierna",100,8.77E-2,{"$f":"F80*(1-Elteq!$F$7)","v":8.77E-2}]
["BIMED","BMBS-21","M16","Záslepka s metrickým závitom M16x1,5 čierna",50,9.3100000000000002E-2,{"$f":"F81*(1-Elteq!$F$7)","v":9.3100000000000002E-2}]
["BIMED","BMBS-22","M20","Záslepka s metrickým závitom M20x1,5 čierna",50,0.1096,{"$f":"F82*(1-Elteq!$F$7)","v":0.1096}]
["BIMED","BMBS-23","M25","Záslepka s metrickým závitom M25x1,5 čierna",25,0.1205,{"$f":"F83*(1-Elteq!$F$7)","v":0.1205}]
["BIMED","BMBS-24","M32","Záslepka s metrickým závitom M32x1,5 čierna",20,0.2082,{"$f":"F84*(1-Elteq!$F$7)","v":0.2082}]
["BIMED","BMBS-25","M40","Záslepka s metrickým závitom M40x1,5 čierna",10,0.54790000000000005,{"$f":"F85*(1-Elteq!$F$7)","v":0.54790000000000005}]
["BIMED","BMBS-26","M50","Záslepka s metrickým závitom M50x1,5 čierna",10,0.92288180250000029,{"$f":"F86*(1-Elteq!$F$7)","v":0.92288180250000029}]
["BIMED","BBS-11","Pg   7","Záslepka Pq 7 svetlošedá",100,3.73E-2,{"$f":"F87*(1-Elteq!$F$7)","v":3.73E-2}]
["BIMED","BBS-12","Pg   9","Záslepka Pq 9 svetlošedá",50,3.73E-2,{"$f":"F88*(1-Elteq!$F$7)","v":3.73E-2}]
["BIMED","BBS-13","Pg 11","Záslepka Pq 11 svetlošedá",50,4.65E-2,{"$f":"F89*(1-Elteq!$F$7)","v":4.65E-2}]
["BIMED","BBS-14","Pg 13.5","Záslepka Pq 13,5 svetlošedá",50,5.04E-2,{"$f":"F90*(1-Elteq!$F$7)","v":5.04E-2},869760632235]
["BIMED","BBS-15","Pg 16","Záslepka Pq 16 svetlošedá",50,5.6099999999999997E-2,{"$f":"F91*(1-Elteq!$F$7)","v":5.6099999999999997E-2},869760632321]
["BIMED","BBS-16","Pg 21","Záslepka Pq 21 svetlošedá",25,7.85E-2,{"$f":"F92*(1-Elteq!$F$7)","v":7.85E-2}]
["BIMED","BBS-17","Pg 29","Záslepka Pq 29 svetlošedá",20,0.1361,{"$f":"F93*(1-Elteq!$F$7)","v":0.1361}]
["BIMED","BBS-18","Pg 36","Záslepka Pq 36 svetlošedá",10,0.22750000000000001,{"$f":"F94*(1-Elteq!$F$7)","v":0.22750000000000001}]
["BIMED","BBS-21","Pg   7","Záslepka Pq 7 čierna",100,3.73E-2,{"$f":"F95*(1-Elteq!$F$7)","v":3.73E-2}]
["BIMED","BBS-22","Pg   9","Záslepka Pq 9 čierna",50,3.73E-2,{"$f":"F96*(1-Elteq!$F$7)","v":3.73E-2}]
["BIMED","BBS-23","Pg 11","Záslepka Pq 11 čierna",50,4.65E-2,{"$f":"F97*(1-Elteq!$F$7)","v":4.65E-2}]
["BIMED","BBS-24","Pg 13.5","Záslepka Pq 13,5 čierna",50,5.04E-2,{"$f":"F98*(1-Elteq!$F$7)","v":5.04E-2}]
["BIMED","BBS-25","Pg 16","Záslepka Pq 16 čierna",50,5.6099999999999997E-2,{"$f":"F99*(1-Elteq!$F$7)","v":5.6099999999999997E-2}]
["BIMED","BBS-26","Pg 21","Záslepka Pq 21 čierna",25,7.85E-2,{"$f":"F100*(1-Elteq!$F$7)","v":7.85E-2}]
["BIMED","BBS-27","Pg 29","Záslepka Pq 29 čierna",20,0.1361,{"$f":"F101*(1-Elteq!$F$7)","v":0.1361}]
["BIMED","BBS-28","Pg 36","Záslepka Pq 36 čierna",10,0.22750000000000001,{"$f":"F102*(1-Elteq!$F$7)","v":0.22750000000000001}]
["BIMED","BPT-21/BPM-2S","PG 7/M12","Zátka z polyamidu čierna",100,5.04E-2,{"$f":"F103*(1-Elteq!$F$7)","v":5.04E-2}]
["BIMED","BPT-22/BPM-E21","PG 9/M16","Zátka z polyamidu čierna",50,5.5899999999999998E-2,{"$f":"F104*(1-Elteq!$F$7)","v":5.5899999999999998E-2}]
["BIMED","BPT-23/BPM-21","PG 11/M16","Zátka z polyamidu čierna",50,6.25E-2,{"$f":"F105*(1-Elteq!$F$7)","v":6.25E-2}]
["BIMED","BPT-24/BPM-22","PG 13,5/M20","Zátka z polyamidu čierna",50,6.7900000000000002E-2,{"$f":"F106*(1-Elteq!$F$7)","v":6.7900000000000002E-2}]
["BIMED","BPT-25/BPM-22L","PG 16/M20","Zátka z polyamidu čierna",50,7.8899999999999998E-2,{"$f":"F107*(1-Elteq!$F$7)","v":7.8899999999999998E-2}]
["BIMED","BPT-26/BPM-E23","PG 21/M25","Zátka z polyamidu čierna",25,8.9915055615000017E-2,{"$f":"F108*(1-Elteq!$F$7)","v":8.9915055615000017E-2}]
["BIMED","BPT-27/BPM-24","PG 29/M32","Zátka z polyamidu čierna",20,0.10441748394000003,{"$f":"F109*(1-Elteq!$F$7)","v":0.10441748394000003}]
["BIMED","BPT-28/BPM-E25","PG 36/M40","Zátka z polyamidu čierna",10,0.118919912265,{"$f":"F110*(1-Elteq!$F$7)","v":0.118919912265}]
["BIMED","BPT-29/BPM-26","PG 42/M50","Zátka z polyamidu čierna",10,0.13184025750000003,{"$f":"F111*(1-Elteq!$F$7)","v":0.13184025750000003}]
["BIMED","BPT-30/BPM-27","PG 48/M63","Zátka z polyamidu čierna",10,0.13975067295000002,{"$f":"F112*(1-Elteq!$F$7)","v":0.13975067295000002}]
["BIMED","BM-0S","M12","Vývodka M12 šedá",100,0.1646,{"$f":"F113*(1-Elteq!$F$7)","v":0.1646},869760630078]
["BIMED","BM-01","M16","Vývodka M16 šedá TL10",50,0.18410000000000001,{"$f":"F114*(1-Elteq!$F$7)","v":0.18410000000000001},869760630040]
["BIMED","BM-01L","M16","Vývodka M16 šedá TL15",50,0.32,{"$f":"F115*(1-Elteq!$F$7)","v":0.32},869760630044]
["BIMED","BM-02","M20","Vývodka M20 šedá TL10 SW24 H29",50,0.22070000000000001,{"$f":"F116*(1-Elteq!$F$7)","v":0.22070000000000001},869760630045]
["BIMED","BM-02L","M20","Vývodka M20 šedá TL15 SW24 H29",50,0.32400000000000001,{"$f":"F117*(1-Elteq!$F$7)","v":0.32400000000000001},869760630050]
["BIMED","BM-03","M20","Vývodka M20 šedá TL 10 SW27 H31",50,0.33750000000000002,{"$f":"F118*(1-Elteq!$F$7)","v":0.33750000000000002},869760630052]
["BIMED","BM-04","M20","Vývodka M20 šedá TL 15 SW27 H31",50,0.35,{"$f":"F119*(1-Elteq!$F$7)","v":0.35},869760630057]
["BIMED","BM-05","M25","Vývodka M25 šedá TL10",25,0.3962,{"$f":"F120*(1-Elteq!$F$7)","v":0.3962},869760630058]
["BIMED","BM-06","M25","Vývodka M25 šedá TL15",25,0.53039999999999998,{"$f":"F121*(1-Elteq!$F$7)","v":0.53039999999999998},869760630065]
["BIMED","BM-07","M32","Vývodka M32 šedá",20,0.98080000000000001,{"$f":"F122*(1-Elteq!$F$7)","v":0.98080000000000001},869760630066]
["BIMED","BM-08","M40","Vývodka M40 šedá",10,1.6251,{"$f":"F123*(1-Elteq!$F$7)","v":1.6251},869760630070]
["BIMED","BM-09","M50","Vývodka M50 šedá","1 (10)",2.5773999999999999,{"$f":"F124*(1-Elteq!$F$7)","v":2.5773999999999999},869760630074]
["BIMED","BM-10","M63","Vývodka M63 šedá","1 (10)",2.8008999999999999,{"$f":"F125*(1-Elteq!$F$7)","v":2.8008999999999999},869760630082]
["BIMED","BM-1S","M12","Vývodka M12 svetlošedá",100,0.1646,{"$f":"F126*(1-Elteq!$F$7)","v":0.1646},869760630127]
["BIMED","BM-11","M16","Vývodka M16 svetlošedá TL10",50,0.18410000000000001,{"$f":"F127*(1-Elteq!$F$7)","v":0.18410000000000001},869760630087]
["BIMED","BM-11L","M16","Vývodka M16 svetlošedá TL15",50,0.32,{"$f":"F128*(1-Elteq!$F$7)","v":0.32},869760630093]
["BIMED","BM-12","M20","Vývodka M20 svetlošedá TL10 SW24 H29",50,0.22070000000000001,{"$f":"F129*(1-Elteq!$F$7)","v":0.22070000000000001},869760630094]
["BIMED","BM-12L","M20","Vývodka M20 svetlošedá TL15 SW24 H29",50,0.32400000000000001,{"$f":"F130*(1-Elteq!$F$7)","v":0.32400000000000001},869760630102]
["BIMED","BM-13","M20","Vývodka M20 svetlošedá TL 10 SW27 H31",50,0.33174999999999999,{"$f":"F131*(1-Elteq!$F$7)","v":0.33174999999999999},869760630103]
["BIMED","BM-14","M20","Vývodka M20 svetlošedá TL 15 SW27 H31",50,0.35,{"$f":"F132*(1-Elteq!$F$7)","v":0.35},869760630107]
["BIMED","BM-15","M25","Vývodka M25 svetlošedá TL10",25,0.3962,{"$f":"F133*(1-Elteq!$F$7)","v":0.3962},869760630108]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"BIMED"},"BM-16","M25","Vývodka M25 svetlošedá TL15",25,0.53039999999999998,{"$f":"F134*(1-Elteq!$F$7)","v":0.53039999999999998},869760630113]
["BIMED","BM-17","M32","Vývodka M32 svetlošedá",20,0.98080000000000001,{"$f":"F135*(1-Elteq!$F$7)","v":0.98080000000000001},869760630114]
["BIMED","BM-18","M40","Vývodka M40 svetlošedá",10,1.6251,{"$f":"F136*(1-Elteq!$F$7)","v":1.6251},869760630118]
["BIMED","BM-19","M50","Vývodka M50 svetlošedá","1 (10)",2.5773999999999999,{"$f":"F137*(1-Elteq!$F$7)","v":2.5773999999999999},869760630122]
["BIMED","BM-20","M63","Vývodka M63 svetlošedá","1 (10)",2.8008999999999999,{"$f":"F138*(1-Elteq!$F$7)","v":2.8008999999999999},869760630132]
["BIMED","BM-2S","M12","Vývodka M12 čierna",100,0.216,{"$f":"F139*(1-Elteq!$F$7)","v":0.216},869760630170]
["BIMED","BM-21","M16","Vývodka M16 čierna TL10",50,0.18410000000000001,{"$f":"F140*(1-Elteq!$F$7)","v":0.18410000000000001},869760630137]
["BIMED","BM-21L","M16","Vývodka M16 čierna TL15",50,0.26483869358693485,{"$f":"F141*(1-Elteq!$F$7)","v":0.26483869358693485},869760630141]
["BIMED","BM-22","M20","Vývodka M20 čierna TL10 SW24 H29",50,0.22070000000000001,{"$f":"F142*(1-Elteq!$F$7)","v":0.22070000000000001},869760630142]
["BIMED","BM-22L","M20","Vývodka M20 čierna TL15 SW24 H29",50,0.32400000000000001,{"$f":"F143*(1-Elteq!$F$7)","v":0.32400000000000001},869760630149]
["BIMED","BM-23","M20","Vývodka M20 čierna TL 10 SW27 H31",50,0.33750000000000002,{"$f":"F144*(1-Elteq!$F$7)","v":0.33750000000000002},869760630150]
["BIMED","BM-24","M20","Vývodka M20 čierna TL 15 SW27 H31",50,0.35,{"$f":"F145*(1-Elteq!$F$7)","v":0.35},869760630152]
["BIMED","BM-25","M25","Vývodka M25 čierna TL10",25,0.3962,{"$f":"F146*(1-Elteq!$F$7)","v":0.3962},869760630154]
["BIMED","BM-26","M25","Vývodka M25 čierna TL15",25,0.53039999999999998,{"$f":"F147*(1-Elteq!$F$7)","v":0.53039999999999998},869760630159]
["BIMED","BM-27","M32","Vývodka M32 čierna",20,0.98080000000000001,{"$f":"F148*(1-Elteq!$F$7)","v":0.98080000000000001},869760630160]
["BIMED","BM-28","M40","Vývodka M40 čierna",10,1.6251,{"$f":"F149*(1-Elteq!$F$7)","v":1.6251},869760630165]
["BIMED","BM-29","M50","Vývodka M50 čierna","1 (10)",2.5773999999999999,{"$f":"F150*(1-Elteq!$F$7)","v":2.5773999999999999},869760630166]
["BIMED","BM-30","M63","Vývodka M63 čierna","1 (10)",2.8008999999999999,{"$f":"F151*(1-Elteq!$F$7)","v":2.8008999999999999},869760630173]
["BIMED","BML-0S","M12","Matica M12 šedá",100,4.4900000000000002E-2,{"$f":"F152*(1-Elteq!$F$7)","v":4.4900000000000002E-2},869760631406]
["BIMED","BML-01","M16","Matica M16 šedá",50,5.7000000000000002E-2,{"$f":"F153*(1-Elteq!$F$7)","v":5.7000000000000002E-2},869760631392]
["BIMED","BML-02","M20","Matica M20 šedá",50,6.25E-2,{"$f":"F154*(1-Elteq!$F$7)","v":6.25E-2},869760631393]
["BIMED","BML-03","M25","Matica M25 šedá",25,9.7500000000000003E-2,{"$f":"F155*(1-Elteq!$F$7)","v":9.7500000000000003E-2},869760631394]
["BIMED","BML-04","M32","Matica M32 šedá",20,0.1173,{"$f":"F156*(1-Elteq!$F$7)","v":0.1173},869760631397]
["BIMED","BML-05","M40","Matica M40 šedá",10,0.33639999999999998,{"$f":"F157*(1-Elteq!$F$7)","v":0.33639999999999998},869760631398]
["BIMED","BML-06","M50","Matica M50 šedá","1 (10)",0.50409999999999999,{"$f":"F158*(1-Elteq!$F$7)","v":0.50409999999999999},869760631402]
["BIMED","BML-07","M63","Mativa M63 šedá","1 (10)",0.56110000000000004,{"$f":"F159*(1-Elteq!$F$7)","v":0.56110000000000004},869760631403]
["BIMED","BML-1S","M12","Matica M12 svetlo šedá",100,4.4900000000000002E-2,{"$f":"F160*(1-Elteq!$F$7)","v":4.4900000000000002E-2},869760631417]
["BIMED","BML-11","M16","Matica M16 svetlo šedá",50,5.7000000000000002E-2,{"$f":"F161*(1-Elteq!$F$7)","v":5.7000000000000002E-2},869760631409]
["BIMED","BML-12","M20","Matica M20 svetlo šedá",50,6.25E-2,{"$f":"F162*(1-Elteq!$F$7)","v":6.25E-2},869760631410]
["BIMED","BML-13","M25","Matica M25 svetlo šedá",25,9.7500000000000003E-2,{"$f":"F163*(1-Elteq!$F$7)","v":9.7500000000000003E-2},869760631412]
["BIMED","BML-14","M32","Matica M32 svetlo šedá",20,0.1173,{"$f":"F164*(1-Elteq!$F$7)","v":0.1173},869760631413]
["BIMED","BML-15","M40","Matica M40 svetlo šedá",10,0.33639999999999998,{"$f":"F165*(1-Elteq!$F$7)","v":0.33639999999999998},869760631414]
["BIMED","BML-16","M50","Matica M50 svetlo šedá","1 (10)",0.50409999999999999,{"$f":"F166*(1-Elteq!$F$7)","v":0.50409999999999999},869760631415]
["BIMED","BML-17","M63","Matica M63 svetlo šedá","1 (10)",0.56110000000000004,{"$f":"F167*(1-Elteq!$F$7)","v":0.56110000000000004},869760631416]
["BIMED","BML-2S","M12","Matica M12 čierna",100,4.4900000000000002E-2,{"$f":"F168*(1-Elteq!$F$7)","v":4.4900000000000002E-2},869760631425]
["BIMED","BML-21","M16","Matica M16 čierna",50,5.7000000000000002E-2,{"$f":"F169*(1-Elteq!$F$7)","v":5.7000000000000002E-2},869760631418]
["BIMED","BML-22","M20","Matica M20 čierna",50,6.25E-2,{"$f":"F170*(1-Elteq!$F$7)","v":6.25E-2},869760631419]
["BIMED","BML-23","M25","Matica M25 čierna",25,9.7500000000000003E-2,{"$f":"F171*(1-Elteq!$F$7)","v":9.7500000000000003E-2},869760631420]
["BIMED","BML-24","M32","Matica M32 čierna",20,0.1173,{"$f":"F172*(1-Elteq!$F$7)","v":0.1173},869760631421]
["BIMED","BML-25","M40","Matica M40 čierna",10,0.33639999999999998,{"$f":"F173*(1-Elteq!$F$7)","v":0.33639999999999998},869760631422]
["BIMED","BML-26","M50","Matica M50 čierna","1 (10)",0.50409999999999999,{"$f":"F174*(1-Elteq!$F$7)","v":0.50409999999999999},869760631423]
["BIMED","BML-27","M63","Matica M63 čierna","1 (10)",0.56110000000000004,{"$f":"F175*(1-Elteq!$F$7)","v":0.56110000000000004},869760631424]
["BIMED","BSSP-11","Pg   7","Špirálová káblová vývodka PG7 svetlošedá",100,0.34080706563749996,{"$f":"F176*(1-Elteq!$F$7)","v":0.34080706563749996},869760631054]
["BIMED","BSSP-12","Pg   9","Špirálová káblová vývodka PG9 svetlošedá",50,0.38866507911000014,{"$f":"F177*(1-Elteq!$F$7)","v":0.38866507911000014},869760631058]
["BIMED","BSSP-13","Pg 11","Špirálová káblová vývodka PG11 svetlošedá",50,0.47567964905999999,{"$f":"F178*(1-Elteq!$F$7)","v":0.47567964905999999},869760631063]
["BIMED","BSSP-14","Pg 13.5","Špirálová káblová vývodka PG13.5 svetlošedá",50,0.53368936236000009,{"$f":"F179*(1-Elteq!$F$7)","v":0.53368936236000009},869760631067]
["BIMED","BSSP-15","Pg 16","Špirálová káblová vývodka PG16 svetlošedá",50,0.66711170295000022,{"$f":"F180*(1-Elteq!$F$7)","v":0.66711170295000022},869760631071]
["BIMED","BSSP-16","Pg 21","Špirálová káblová vývodka PG21 svetlošedá",25,0.99341634026250003,{"$f":"F181*(1-Elteq!$F$7)","v":0.99341634026250003},869760631075]
["BIMED","BSSP-21","Pg   7","Špirálová káblová vývodka PG7 čierna",100,0.34080706563749996,{"$f":"F182*(1-Elteq!$F$7)","v":0.34080706563749996},869760631078]
["BIMED","BSSP-22","Pg   9","Špirálová káblová vývodka PG9 čierna",50,0.38866507911000014,{"$f":"F183*(1-Elteq!$F$7)","v":0.38866507911000014},869760631082]
["BIMED","BSSP-23","Pg 11","Špirálová káblová vývodka PG11 čierna",50,0.47567964905999999,{"$f":"F184*(1-Elteq!$F$7)","v":0.47567964905999999},869760631085]
["BIMED","BSSP-24","Pg 13.5","Špirálová káblová vývodka PG13.5 čierna",50,0.53368936236000009,{"$f":"F185*(1-Elteq!$F$7)","v":0.53368936236000009},869760631089]
["BIMED","BSSP-25","Pg 16","Špirálová káblová vývodka PG16 čierna",50,0.66711170295000022,{"$f":"F186*(1-Elteq!$F$7)","v":0.66711170295000022},869760631091]
["BIMED","BSSP-26","Pg 21","Špirálová káblová vývodka PG21 čierna",25,0.99341634026250003,{"$f":"F187*(1-Elteq!$F$7)","v":0.99341634026250003},869760631093]
["BIMED","BM-EN-1S","M12","Vývodka Euro Metric  M12 svetlošedá",100,0.21782647344150008,{"$f":"F188*(1-Elteq!$F$7)","v":0.21782647344150008}]
["BIMED","BM-EN-11","M16","Vývodka Euro Metric M16 svetlošedá",50,0.24364079586000009,{"$f":"F189*(1-Elteq!$F$7)","v":0.24364079586000009},869760630222]
["BIMED","BM-EN-12","M20","Vývodka Euro Metric M20 svetlošedá",50,0.29207890646550011,{"$f":"F190*(1-Elteq!$F$7)","v":0.29207890646550011}]
["BIMED","BM-EN-13","M25","Vývodka Euro Metric M25 svetlošedá",25,0.52440780823200017,{"$f":"F191*(1-Elteq!$F$7)","v":0.52440780823200017},869760630226]
["BIMED","BM-EN-14","M32","Vývodka Euro Metric M32 svetlošedá",20,1.2979673350875003,{"$f":"F192*(1-Elteq!$F$7)","v":1.2979673350875003},869760630229]
["BIMED","BM-EN-15","M40","Vývodka Euro Metric M40 svetlošedá",10,2.1507101205975001,{"$f":"F193*(1-Elteq!$F$7)","v":2.1507101205975001},869760630232]
["BIMED","BM-EN-16","M50","Vývodka Euro Metric M50 svetlošedá","1 (10)",3.4109711420400015,{"$f":"F194*(1-Elteq!$F$7)","v":3.4109711420400015}]
["BIMED","BM-EN-17","M63","Vývodka Euro Metric M63 svetlošedá","1 (10)",3.7068206798699999,{"$f":"F195*(1-Elteq!$F$7)","v":3.7068206798699999}]
["BIMED","BM-XS","M12","Vývodka M12 EEX čierna",100,0.43830000000000002,{"$f":"F196*(1-Elteq!$F$7)","v":0.43830000000000002},869760631180]
["BIMED","BM-X1","M16","Vývodka M16 EEX čierna",50,0.50409999999999999,{"$f":"F197*(1-Elteq!$F$7)","v":0.50409999999999999},869760631153]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"BIMED"},"BM-X1L","M16","Vývodka M16 EEX čierna predĺžený záv.",50,0.50409999999999999,{"$f":"F198*(1-Elteq!$F$7)","v":0.50409999999999999},869760631155]
["BIMED","BM-X2","M20","Vývodka M20 EEX čierna",50,0.67279999999999995,{"$f":"F199*(1-Elteq!$F$7)","v":0.67279999999999995},869760631156]
["BIMED","BM-X2L","M20","Vývodka M20 EEX čierna predĺženný záv.",50,0.67279999999999995,{"$f":"F200*(1-Elteq!$F$7)","v":0.67279999999999995},869760631159]
["BIMED","BM-X3","M20","Vývodka M20 EEX čierna",50,0.89859999999999995,{"$f":"F201*(1-Elteq!$F$7)","v":0.89859999999999995},869760631160]
["BIMED","BM-X4","M20","Vývodka M20 EEX čierna",50,0.92049999999999998,{"$f":"F202*(1-Elteq!$F$7)","v":0.92049999999999998},869760631163]
["BIMED","BM-X5","M25","Vývodka M25 EEX čierna",25,0.95340000000000003,{"$f":"F203*(1-Elteq!$F$7)","v":0.95340000000000003},869760631167]
["BIMED","BM-X6","M25","Vývodka M25 EEX čierna",25,1.5561,{"$f":"F204*(1-Elteq!$F$7)","v":1.5561},869760631171]
["BIMED","BM-X7","M32","Vývodka M32 EEX čierna",20,2.4108000000000001,{"$f":"F205*(1-Elteq!$F$7)","v":2.4108000000000001},869760631173]
["BIMED","BM-X8","M40","Vývodka M40 EEX čierna",10,2.802,{"$f":"F206*(1-Elteq!$F$7)","v":2.802},869760631175]
["BIMED","BM-X9","M50","Vývodka M50 EEX čierna","1 (10)",3.9220000000000002,{"$f":"F207*(1-Elteq!$F$7)","v":3.9220000000000002},869760631178]
["BIMED","BM-X0","M63","Vývodka M63 EEX čierna","1 (10)",4.2024999999999997,{"$f":"F208*(1-Elteq!$F$7)","v":4.2024999999999997},869760631151]
["BIMED","BMSP-1S","M12","Vývodka špirálová M12 svetlo šedá",100,0.3594,{"$f":"F209*(1-Elteq!$F$7)","v":0.3594},869760630459]
["BIMED","BMSP-11","M16","Vývodka špirálová M16 svetlo šedá",50,0.4274,{"$f":"F210*(1-Elteq!$F$7)","v":0.4274},869760630450]
["BIMED","BMSP-12","M20","Vývodka špirálová M20 svetlo šedá TL10 SW24 H95",50,0.48220000000000002,{"$f":"F211*(1-Elteq!$F$7)","v":0.48220000000000002},869760630452]
["BIMED","BMSP-12L","M20","Vývodka špirálová M20 svetlo šedá TL15 SW24 H95",50,0.78400000000000003,{"$f":"F212*(1-Elteq!$F$7)","v":0.78400000000000003},869760630454]
["BIMED","BMSP-13","M20","Vývodka špirálová M20 svetlo šedá TL10 SW27 H105",50,0.61799999999999999,{"$f":"F213*(1-Elteq!$F$7)","v":0.61799999999999999},869760630455]
["BIMED","BMSP-14","M20","Vývodka špirálová M20 svetlo šedá TL15 SW27 H105",50,0.74165354112726545,{"$f":"F214*(1-Elteq!$F$7)","v":0.74165354112726545},869760630456]
["BIMED","BMSP-15","M25","Vývodka špirálová M25 svetlo šedá",25,0.88539999999999996,{"$f":"F215*(1-Elteq!$F$7)","v":0.88539999999999996},869760630458]
["BIMED","BMSP-2S","M12","Vývodka špirálová M16 čierna",100,0.3594,{"$f":"F216*(1-Elteq!$F$7)","v":0.3594},869760630469]
["BIMED","BMSP-21","M16","Vývodka špirálová M16 čierna",50,0.4274,{"$f":"F217*(1-Elteq!$F$7)","v":0.4274},869760630461]
["BIMED","BMSP-22","M20","Vývodka špirálová M20 čierna TL10 SW24 H95",50,0.48220000000000002,{"$f":"F218*(1-Elteq!$F$7)","v":0.48220000000000002},869760630465]
["BIMED","BMSP-22L","M20","Vývodka špirálová M20 čierna TL15 SW24 H95",50,0.78400000000000003,{"$f":"F219*(1-Elteq!$F$7)","v":0.78400000000000003}]
["BIMED","BMSP-24","M20","Vývodka špirálová M20 čierna TL15 SW27 H105",50,0.61799999999999999,{"$f":"F220*(1-Elteq!$F$7)","v":0.61799999999999999},869760630467]
["BIMED","BMSP-25","M25","Vývodka špirálová M25 čierna",25,0.88539999999999996,{"$f":"F221*(1-Elteq!$F$7)","v":0.88539999999999996},869760630468]
["BIMED","BBVP-0S","PG 7","Ventilačná ucpávka z nerezovej ocele PG7",1,6.5920128750000018,{"$f":"F222*(1-Elteq!$F$7)","v":6.5920128750000018}]
["BIMED","BBVP-01","M12X1,5","Ventilačná ucpávka z nerezovej ocele M12",1,6.5920128750000018,{"$f":"F223*(1-Elteq!$F$7)","v":6.5920128750000018}]
["BIMED","BVPA-11","M12x1,0","Ventilačná ucpávka z polyamidu M12x1.0 svetlošedá",1,1.4835984176475003,{"$f":"F224*(1-Elteq!$F$7)","v":1.4835984176475003}]
["BIMED","BVPA-21","M12x1,0","Ventilačná ucpávka z polyamidu M12x1.0 čierna",1,1.4835984176475003,{"$f":"F225*(1-Elteq!$F$7)","v":1.4835984176475003}]
["BIMED","BVPB-11","M12X1,5","Ventilačná ucpávka z polyamidu M12x1.5 svetlošedá TL6.0",1,1.4835984176475003,{"$f":"F226*(1-Elteq!$F$7)","v":1.4835984176475003}]
["BIMED","BVPB-21","M12X1,5","Ventilačná ucpávka z polyamidu M12x1.5 čierna TL 6.0",1,1.4835984176475003,{"$f":"F227*(1-Elteq!$F$7)","v":1.4835984176475003}]
["BIMED","BVPB-11L","M12X1,5","Ventilačná ucpávka z polyamidu M12x1.5 svetlošedá TL10",1,1.4835984176475003,{"$f":"F228*(1-Elteq!$F$7)","v":1.4835984176475003}]
["BIMED","BVPB-21L","M12X1,5","Ventilačná ucpávka z polyamidu M12x1.5 čierna TL 10",1,1.4835984176475003,{"$f":"F229*(1-Elteq!$F$7)","v":1.4835984176475003}]
["BIMED","BSEM-01","Pg   7","Vývodka mosadzná pre tienené káble Pg7",1,2.1541999999999999,{"$f":"F230*(1-Elteq!$F$7)","v":2.1541999999999999},869760631756]
["BIMED","BSEM-02","Pg   9","Vývodka mosadzná pre tienené káble Pg9",1,2.3872,{"$f":"F231*(1-Elteq!$F$7)","v":2.3872},869760631757]
["BIMED","BSEM-03","Pg 11","Vývodka mosadzná pre tienené káble Pg11",1,2.5838999999999999,{"$f":"F232*(1-Elteq!$F$7)","v":2.5838999999999999},869760631758]
["BIMED","BSEM-04","Pg 13.5","Vývodka mosadzná pre tienené káble Pg13,5",1,3.0333999999999999,{"$f":"F233*(1-Elteq!$F$7)","v":3.0333999999999999},869760631759]
["BIMED","BSEM-05","Pg 16","Vývodka mosadzná pre tienené káble Pg16",1,3.1736,{"$f":"F234*(1-Elteq!$F$7)","v":3.1736},869760631760]
["BIMED","BSEM-06","Pg 21","Vývodka mosadzná pre tienené káble Pg21",1,4.4375999999999998,{"$f":"F235*(1-Elteq!$F$7)","v":4.4375999999999998},869760631761]
["BIMED","BSEM-07","Pg 29","Vývodka mosadzná pre tienené káble Pg29",1,6.9090999999999996,{"$f":"F236*(1-Elteq!$F$7)","v":6.9090999999999996},869760631762]
["BIMED","BSEM-08","Pg 36","Vývodka mosadzná pre tienené káble Pg36",1,12.2789,{"$f":"F237*(1-Elteq!$F$7)","v":12.2789},869760631763]
["BIMED","BSEM-09","Pg 42","Vývodka mosadzná pre tienené káble Pg42",1,19.6738,{"$f":"F238*(1-Elteq!$F$7)","v":19.6738},869760631764]
["BIMED","BSEM-10","Pg 48","Vývodka mosadzná pre tienené káble Pg48",1,23.867100000000001,{"$f":"F239*(1-Elteq!$F$7)","v":23.867100000000001},869760631765]
["BIMED","BMEM-0S","M12","Vývodka mosadzná pre tienené kab. M12",1,2.6400999999999999,{"$f":"F240*(1-Elteq!$F$7)","v":2.6400999999999999},869760631727]
["BIMED","BMEM-01","M16","Vývodka mosadzná pre tienené kab. M16",1,2.9209000000000001,{"$f":"F241*(1-Elteq!$F$7)","v":2.9209000000000001},869760631719]
["BIMED","BMEM-02","M20","Vývodka mosadzná pre tienené kab. M20",1,3.4264999999999999,{"$f":"F242*(1-Elteq!$F$7)","v":3.4264999999999999},869760631721]
["BIMED","BMEM-03","M25","Vývodka mosadzná pre tienené kab. M25",1,4.3813000000000004,{"$f":"F243*(1-Elteq!$F$7)","v":4.3813000000000004},869760631722]
["BIMED","BMEM-04","M32","Vývodka mosadzná pre tienené kab. M32",1,5.4486999999999997,{"$f":"F244*(1-Elteq!$F$7)","v":5.4486999999999997},869760631723]
["BIMED","BMEM-05","M40","Vývodka mosadzná pre tienené kab. M40",1,8.4002999999999997,{"$f":"F245*(1-Elteq!$F$7)","v":8.4002999999999997},869760631724]
["BIMED","BMEM-06","M50","Vývodka mosadzná pre tienené kab. M50",1,14.733700000000001,{"$f":"F246*(1-Elteq!$F$7)","v":14.733700000000001},869760631725]
["BIMED","BMEM-07","M63","Vývodka mosadzná pre tienené kab. M63",1,21.540099999999999,{"$f":"F247*(1-Elteq!$F$7)","v":21.540099999999999},869760631726]
["BIMED","BSBC-01","Pg   7","Vývodka mosadzná Pg7",1,0.92010000000000003,{"$f":"F248*(1-Elteq!$F$7)","v":0.92010000000000003},869760631567]
["BIMED","BSBC-02","Pg   9","Vývodka mosadzná Pg9",1,1.1279999999999999,{"$f":"F249*(1-Elteq!$F$7)","v":1.1279999999999999},869760631568]
["BIMED","BSBC-03","Pg 11","Vývodka mosadzná Pg11",1,1.3394999999999999,{"$f":"F250*(1-Elteq!$F$7)","v":1.3394999999999999},869760631569]
["BIMED","BSBC-04","Pg 13.5","Vývodka mosadzná Pg13,5",1,1.5509999999999999,{"$f":"F251*(1-Elteq!$F$7)","v":1.5509999999999999},869760631570]
["BIMED","BSBC-05","Pg 16","Vývodka mosadzná Pg16",1,1.6214999999999999,{"$f":"F252*(1-Elteq!$F$7)","v":1.6214999999999999},869760631571]
["BIMED","BSBC-06","Pg 21","Vývodka mosadzná Pg21",1,2.7141999999999999,{"$f":"F253*(1-Elteq!$F$7)","v":2.7141999999999999},869760631572]
["BIMED","BSBC-07","Pg 29","Vývodka mosadzná Pg29",1,4.0538999999999996,{"$f":"F254*(1-Elteq!$F$7)","v":4.0538999999999996},869760631573]
["BIMED","BSBC-08","Pg 36","Vývodka mosadzná Pg36",1,8.6504999999999992,{"$f":"F255*(1-Elteq!$F$7)","v":8.6504999999999992},869760631574]
["BIMED","BSBC-09","Pg 42","Vývodka mosadzná Pg42",1,14.8687,{"$f":"F256*(1-Elteq!$F$7)","v":14.8687},869760631575]
["BIMED","BSBC-10","Pg 48","Vývodka mosadzná Pg48",1,19.8249,{"$f":"F257*(1-Elteq!$F$7)","v":19.8249},869760631576]
["BIMED","BSEL-01","Pg   7","Matica mosadzná pre tienene káble Pg7",1,0.1439,{"$f":"F258*(1-Elteq!$F$7)","v":0.1439},869760631811]
["BIMED","BSEL-02","Pg   9","Matica mosadzná pre tienene káble Pg9",1,0.15229999999999999,{"$f":"F259*(1-Elteq!$F$7)","v":0.15229999999999999},869760631812]
["BIMED","BSEL-03","Pg 11","Matica mosadzná pre tienene káble Pg11",1,0.1636,{"$f":"F260*(1-Elteq!$F$7)","v":0.1636},869760631813]
["BIMED","BSEL-04","Pg 13.5","Matica mosadzná pre tienene káble Pg13,5",1,0.18099999999999999,{"$f":"F261*(1-Elteq!$F$7)","v":0.18099999999999999},869760631814]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"BIMED"},"BSEL-05","Pg 16","Matica mosadzná pre tienene káble Pg16",1,0.20960000000000001,{"$f":"F262*(1-Elteq!$F$7)","v":0.20960000000000001},869760631815]
["BIMED","BSEL-06","Pg 21","Matica mosadzná pre tienene káble Pg21",1,0.33029999999999998,{"$f":"F263*(1-Elteq!$F$7)","v":0.33029999999999998},869760631816]
["BIMED","BSEL-07","Pg 29","Matica mosadzná pre tienene káble Pg29",1,0.56000000000000005,{"$f":"F264*(1-Elteq!$F$7)","v":0.56000000000000005},869760631817]
["BIMED","BSEL-08","Pg 36","Matica mosadzná pre tienene káble Pg36",1,0.89039999999999997,{"$f":"F265*(1-Elteq!$F$7)","v":0.89039999999999997},869760631818]
["BIMED","BSEL-09","Pg 42","Matica mosadzná pre tienene káble Pg42",1,2.0104000000000002,{"$f":"F266*(1-Elteq!$F$7)","v":2.0104000000000002},869760631819]
["BIMED","BSEL-10","Pg 48","Matica mosadzná pre tienene káble Pg48",1,2.0676000000000001,{"$f":"F267*(1-Elteq!$F$7)","v":2.0676000000000001},869760631820]
["BIMED","BMEL-01","M12","Matica mosazdzná pre tienene kab. M12",1,0.32200000000000001,{"$f":"F268*(1-Elteq!$F$7)","v":0.32200000000000001},869760631803]
["BIMED","BMEL-02","M16","Matica mosazdzná pre tienene kab. M16",1,0.34499999999999997,{"$f":"F269*(1-Elteq!$F$7)","v":0.34499999999999997},869760631804]
["BIMED","BMEL-03","M20","Matica mosazdzná pre tienene kab. M20",1,0.38740000000000002,{"$f":"F270*(1-Elteq!$F$7)","v":0.38740000000000002},869760631805]
["BIMED","BMEL-04","M25","Matica mosazdzná pre tienene kab. M25",1,0.65210000000000001,{"$f":"F271*(1-Elteq!$F$7)","v":0.65210000000000001},869760631806]
["BIMED","BMEL-05","M32","Matica mosazdzná pre tienene kab. M32",1,0.95309999999999995,{"$f":"F272*(1-Elteq!$F$7)","v":0.95309999999999995},869760631807]
["BIMED","BMEL-06","M40","Matica mosazdzná pre tienene kab. M40",1,1.6655,{"$f":"F273*(1-Elteq!$F$7)","v":1.6655},869760631808]
["BIMED","BMEL-07","M50","Matica mosazdzná pre tienene kab. M50",1,4.5087000000000002,{"$f":"F274*(1-Elteq!$F$7)","v":4.5087000000000002},869760631809]
["BIMED","BMEL-08","M63","Matica mosazdzná pre tienene kab. M63",1,4.8823999999999996,{"$f":"F275*(1-Elteq!$F$7)","v":4.8823999999999996},869760631810]
["BIMED","BSL-01","Pg   7","Matica mosadzná Pg7",1,9.0399999999999994E-2,{"$f":"F276*(1-Elteq!$F$7)","v":9.0399999999999994E-2},869760631656]
["BIMED","BSL-02","Pg   9","Matica mosadzná Pg9",1,9.5600000000000004E-2,{"$f":"F277*(1-Elteq!$F$7)","v":9.5600000000000004E-2},869760631657]
["BIMED","BSL-03","Pg 11","Matica mosadzná Pg11",1,0.1027,{"$f":"F278*(1-Elteq!$F$7)","v":0.1027},869760631658]
["BIMED","BSL-04","Pg 13.5","Matica mosadzná Pg13,5",1,0.11360000000000001,{"$f":"F279*(1-Elteq!$F$7)","v":0.11360000000000001},869760631659]
["BIMED","BSL-05","Pg 16","Matica mosadzná Pg16",1,0.13159999999999999,{"$f":"F280*(1-Elteq!$F$7)","v":0.13159999999999999},869760631661]
["BIMED","BSL-06","Pg 21","Matica mosadzná Pg21",1,0.20730000000000001,{"$f":"F281*(1-Elteq!$F$7)","v":0.20730000000000001},869760631663]
["BIMED","BSL-07","Pg 29","Matica mosadzná Pg29",1,0.35149999999999998,{"$f":"F282*(1-Elteq!$F$7)","v":0.35149999999999998},869760631665]
["BIMED","BSL-08","Pg 36","Matica mosadzná Pg36",1,0.77739999999999998,{"$f":"F283*(1-Elteq!$F$7)","v":0.77739999999999998},869760631666]
["BIMED","BSL-09","Pg 42","Matica mosadzná Pg42",1,1.2617,{"$f":"F284*(1-Elteq!$F$7)","v":1.2617},869760631668]
["BIMED","BSL-10","Pg 48","Matica mosadzná Pg48",1,1.2975000000000001,{"$f":"F285*(1-Elteq!$F$7)","v":1.2975000000000001},869760631669]
["BIMED","BMBC-0S","M12","Vývodka mosadzná M12",1,1.3044,{"$f":"F286*(1-Elteq!$F$7)","v":1.3044},869760631503]
["BIMED","BMBC-01","M16","Vývodka mosadzná M16",1,1.4804999999999999,{"$f":"F287*(1-Elteq!$F$7)","v":1.4804999999999999},869760631492]
["BIMED","BMBC-02","M20","Vývodka mosadzná M20",1,1.8684000000000001,{"$f":"F288*(1-Elteq!$F$7)","v":1.8684000000000001},869760631494]
["BIMED","BMBC-03","M25","Vývodka mosadzná M25",1,2.3262999999999998,{"$f":"F289*(1-Elteq!$F$7)","v":2.3262999999999998},869760631495]
["BIMED","BMBC-04","M32","Vývodka mosadzná M32",1,3.3841000000000001,{"$f":"F290*(1-Elteq!$F$7)","v":3.3841000000000001},869760631496]
["BIMED","BMBC-05","M40","Vývodka mosadzná M40",1,5.0479000000000003,{"$f":"F291*(1-Elteq!$F$7)","v":5.0479000000000003},869760631497]
["BIMED","BMBC-06","M50","Vývodka mosadzná M50",1,8.8690999999999995,{"$f":"F292*(1-Elteq!$F$7)","v":8.8690999999999995},869760631501]
["BIMED","BMBC-07","M63","Vývodka mosadzná M63 TL14 SW1-64 SW2-68 ",1,16.2224,{"$f":"F293*(1-Elteq!$F$7)","v":16.2224},869760631502]
["BIMED","BMBC-07S","M63","Vývodka mosadzná M63 TL10 SW1-75 SW2-75",1,29.795999999999999,{"$f":"F294*(1-Elteq!$F$7)","v":29.795999999999999}]
["BIMED","BMBL-01","M12","Matica mosadzná M12",1,0.2021,{"$f":"F295*(1-Elteq!$F$7)","v":0.2021},869760631644]
["BIMED","BMBL-02","M16","Matica mosadzná M16",1,0.2165,{"$f":"F296*(1-Elteq!$F$7)","v":0.2165},869760631645]
["BIMED","BMBL-03","M20","Matica mosadzná M20",1,0.24329999999999999,{"$f":"F297*(1-Elteq!$F$7)","v":0.24329999999999999},869760631647]
["BIMED","BMBL-04","M25","Matica mosadzná M25",1,0.40920000000000001,{"$f":"F298*(1-Elteq!$F$7)","v":0.40920000000000001},869760631648]
["BIMED","BMBL-05","M32","Matica mosadzná M32",1,0.59809999999999997,{"$f":"F299*(1-Elteq!$F$7)","v":0.59809999999999997},869760631650]
["BIMED","BMBL-06","M40","Matica mosadzná M40",1,1.0451999999999999,{"$f":"F300*(1-Elteq!$F$7)","v":1.0451999999999999},869760631651]
["BIMED","BMBL-07","M50","Matica mosadzná M50",1,2.8294999999999999,{"$f":"F301*(1-Elteq!$F$7)","v":2.8294999999999999},869760631652]
["BIMED","BMBL-08","M63","Matica mosadzná M63",1,3.0640000000000001,{"$f":"F302*(1-Elteq!$F$7)","v":3.0640000000000001},869760631653]
["BIMED","BSBE-01","Pg   7","Vývodka mosadzná s predlženým závitom Pg7",1,1.0134000000000001,{"$f":"F303*(1-Elteq!$F$7)","v":1.0134000000000001},869760631596]
["BIMED","BSBE-02","Pg   9","Vývodka mosadzná s predlženým závitom Pg9",1,1.2407999999999999,{"$f":"F304*(1-Elteq!$F$7)","v":1.2407999999999999},869760631599]
["BIMED","BSBE-03","Pg 11","Vývodka mosadzná s predlženým závitom Pg11",1,1.4734,{"$f":"F305*(1-Elteq!$F$7)","v":1.4734},869760631601]
["BIMED","BSBE-04","Pg 13.5","Vývodka mosadzná s predlženým závitom Pg13,5",1,1.7062999999999999,{"$f":"F306*(1-Elteq!$F$7)","v":1.7062999999999999},869760631603]
["BIMED","BSBE-05","Pg 16","Vývodka mosadzná s predlženým závitom Pg16",1,1.7837000000000001,{"$f":"F307*(1-Elteq!$F$7)","v":1.7837000000000001},869760631605]
["BIMED","BSBE-06","Pg 21","Vývodka mosadzná s predlženým závitom Pg21",1,2.9857,{"$f":"F308*(1-Elteq!$F$7)","v":2.9857},869760631607]
["BIMED","BSBE-07","Pg 29","Vývodka mosadzná s predlženým závitom Pg29",1,4.4592000000000001,{"$f":"F309*(1-Elteq!$F$7)","v":4.4592000000000001},869760631609]
["BIMED","BSBE-08","Pg 36","Vývodka mosadzná s predlženým závitom Pg36",1,9.516,{"$f":"F310*(1-Elteq!$F$7)","v":9.516},869760631611]
["BIMED","BSBE-09","Pg 42","Vývodka mosadzná s predlženým závitom Pg42",1,16.356300000000001,{"$f":"F311*(1-Elteq!$F$7)","v":16.356300000000001},869760631612]
["BIMED","BSBE-10","Pg 48","Vývodka mosadzná s predlženým závitom Pg48",1,21.8079,{"$f":"F312*(1-Elteq!$F$7)","v":21.8079},869760631613]
["BIMED","BMBE-0S","M12","Vývodka mosadzná s predĺženým závitom M12",1,1.4347000000000001,{"$f":"F313*(1-Elteq!$F$7)","v":1.4347000000000001},869760631537]
["BIMED","BMBE-01","M16","Vývodka mosadzná s predĺženým závitom M16",1,1.6286,{"$f":"F314*(1-Elteq!$F$7)","v":1.6286},869760631524]
["BIMED","BMBE-02","M20","Vývodka mosadzná s predĺženým závitom M20",1,2.0552000000000001,{"$f":"F315*(1-Elteq!$F$7)","v":2.0552000000000001},869760631527]
["BIMED","BMBE-03","M25","Vývodka mosadzná s predĺženým závitom M25",1,2.5592000000000001,{"$f":"F316*(1-Elteq!$F$7)","v":2.5592000000000001},869760631529]
["BIMED","BMBE-04","M32","Vývodka mosadzná s predĺženým závitom M32",1,3.7225999999999999,{"$f":"F317*(1-Elteq!$F$7)","v":3.7225999999999999},869760631531]
["BIMED","BMBE-05","M40","Vývodka mosadzná s predĺženým závitom M40",1,5.5537000000000001,{"$f":"F318*(1-Elteq!$F$7)","v":5.5537000000000001},869760631532]
["BIMED","BMBE-06","M50","Vývodka mosadzná s predĺženým závitom M50",1,9.7574000000000005,{"$f":"F319*(1-Elteq!$F$7)","v":9.7574000000000005},869760631534]
["BIMED","BMBE-07","M63","Vývodka mosadzná s predĺženým závitom M63",1,17.845600000000001,{"$f":"F320*(1-Elteq!$F$7)","v":17.845600000000001},869760631536]
["BIMED","BMEN-0S","M12","Vývodka mosadzná pre tienené kab. Predlž. závit M12",1,2.9039000000000001,{"$f":"F321*(1-Elteq!$F$7)","v":2.9039000000000001},869760631752]
["BIMED","BMEN-01","M16","Vývodka mosadzná pre tienené kab. Predlž. závit M16",1,3.2128999999999999,{"$f":"F322*(1-Elteq!$F$7)","v":3.2128999999999999},869760631744]
["BIMED","BMEN-02","M20","Vývodka mosadzná pre tienené kab. Predlž. závit M20",1,3.7690000000000001,{"$f":"F323*(1-Elteq!$F$7)","v":3.7690000000000001},869760631746]
["BIMED","BMEN-03","M25","Vývodka mosadzná pre tienené kab. Predlž. závit M25",1,4.8193999999999999,{"$f":"F324*(1-Elteq!$F$7)","v":4.8193999999999999},869760631747]
["BIMED","BMEN-04","M32","Vývodka mosadzná pre tienené kab. Predlž. závit M32",1,5.9934000000000003,{"$f":"F325*(1-Elteq!$F$7)","v":5.9934000000000003},869760631748]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"BIMED"},"BMEN-05","M40","Vývodka mosadzná pre tienené kab. Predlž. závit M40",1,9.2401,{"$f":"F326*(1-Elteq!$F$7)","v":9.2401},869760631749]
["BIMED","BMEN-06","M50","Vývodka mosadzná pre tienené kab. Predlž. závit M50",1,16.208200000000001,{"$f":"F327*(1-Elteq!$F$7)","v":16.208200000000001},869760631750]
["BIMED","BMEN-07","M63","Vývodka mosadzná pre tienené kab. Predlž. závit M63",1,23.694299999999998,{"$f":"F328*(1-Elteq!$F$7)","v":23.694299999999998},869760631751]
["BIMED","BSEN-01","Pg   7","Vývodka mosadzná pre tienené káble predlžený závit Pg7",1,2.3704999999999998,{"$f":"F329*(1-Elteq!$F$7)","v":2.3704999999999998}]
["BIMED","BSEN-02","Pg   9","Vývodka mosadzná pre tienené káble predlžený závit Pg9",1,2.6259000000000001,{"$f":"F330*(1-Elteq!$F$7)","v":2.6259000000000001},869760631776]
["BIMED","BSEN-03","Pg 11","Vývodka mosadzná pre tienené káble predlžený závit Pg11",1,2.8422000000000001,{"$f":"F331*(1-Elteq!$F$7)","v":2.8422000000000001},869760631778]
["BIMED","BSEN-04","Pg 13.5","Vývodka mosadzná pre tienené káble predlžený závit Pg13,5",1,3.3365999999999998,{"$f":"F332*(1-Elteq!$F$7)","v":3.3365999999999998},869760631780]
["BIMED","BSEN-05","Pg 16","Vývodka mosadzná pre tienené káble predlžený závit Pg16",1,3.4910000000000001,{"$f":"F333*(1-Elteq!$F$7)","v":3.4910000000000001},869760631782]
["BIMED","BSEN-06","Pg 21","Vývodka mosadzná pre tienené káble predlžený závit Pg21",1,4.8813000000000004,{"$f":"F334*(1-Elteq!$F$7)","v":4.8813000000000004},869760631784]
["BIMED","BSEN-07","Pg 29","Vývodka mosadzná pre tienené káble predlžený závit Pg29",1,7.5998999999999999,{"$f":"F335*(1-Elteq!$F$7)","v":7.5998999999999999},869760631785]
["BIMED","BSSC-01","Pg   7","Káblová vývodká s PG závitom PG7 nerezová AISI 303",50,11.470102402500004,{"$f":"F336*(1-Elteq!$F$7)","v":11.470102402500004},869760631614]
["BIMED","BSSC-02","Pg   9","Káblová vývodka s PG závitom PG9 nerezová AISI 303",50,13.975067295000001,{"$f":"F337*(1-Elteq!$F$7)","v":13.975067295000001},869760631615]
["BIMED","BSSC-03","Pg 11","Káblová vývodka s PG závitom PG11 nerezová AISI 303",50,15.557150385000002,{"$f":"F338*(1-Elteq!$F$7)","v":15.557150385000002},869760631616]
["BIMED","BSSC-04","Pg 13.5","Káblová vývodka s PG závitom PG13.5 nerezová AISI 303",50,16.480032187500001,{"$f":"F339*(1-Elteq!$F$7)","v":16.480032187500001},869760631617]
["BIMED","BSSC-05","Pg 16","Káblová vývodka s PG závitom PG16 nerezová AISI 303",25,17.139233475000001,{"$f":"F340*(1-Elteq!$F$7)","v":17.139233475000001},869760631618]
["BIMED","BSSC-06","Pg 21","Káblová vývodka s PG závitom PG21 nerezová AISI 303",25,25.313329440000004,{"$f":"F341*(1-Elteq!$F$7)","v":25.313329440000004},869760631619]
["BIMED","BSSC-07","Pg 29","Káblová vývodka s PG závitom PG29 nerezová AISI 303",20,32.960064375000002,{"$f":"F342*(1-Elteq!$F$7)","v":32.960064375000002},869760631620]
["BIMED","BSSC-08","Pg 36","Káblová vývodka s PG závitom PG36 nerezová AISI 303",15,41.925201885000007,{"$f":"F343*(1-Elteq!$F$7)","v":41.925201885000007},869760631621]
["BIMED","BSSC-09","Pg 42","Káblová vývodka s PG závitom PG42 nerezová AISI 303",12,79.104154500000007,{"$f":"F344*(1-Elteq!$F$7)","v":79.104154500000007},869760631622]
["BIMED","BSSC-10","Pg 48","Káblová vývodka s PG závitom PG48 nerezová AISI 303",12,94.924985400000025,{"$f":"F345*(1-Elteq!$F$7)","v":94.924985400000025},869760631623]
["BIMED","BMSC-0S","M12","Káblová vývodka s metrickým závitom M12 nerezová AISI 303",50,11.470102402500004,{"$f":"F346*(1-Elteq!$F$7)","v":11.470102402500004},869760631543]
["BIMED","BMSC-01","M16","Káblová vývodka s metrickým závitom M16 nerezová AISI 303",50,11.733782917500005,{"$f":"F347*(1-Elteq!$F$7)","v":11.733782917500005},869760631538]
["BIMED","BMSC-02","M20","Káblová vývodka s metrickým závitom M20 nerezová AISI 303",50,15.161629612500001,{"$f":"F348*(1-Elteq!$F$7)","v":15.161629612500001},869760631539]
["BIMED","BMSC-03","M25","Káblová vývodka s metrickým závitom M25 nerezová AISI 303",25,16.348191930000002,{"$f":"F349*(1-Elteq!$F$7)","v":16.348191930000002},869760631540]
["BIMED","BMSC-04","M32","Káblová vývodka s metrickým závitom M32 nerezová AISI 303",25,20.039719140000003,{"$f":"F350*(1-Elteq!$F$7)","v":20.039719140000003},869760631541]
["BIMED","BMSC-05","M40","Káblová vývodka s metrickým závitom M40 nerezová AISI 303",20,34.805827980000011,{"$f":"F351*(1-Elteq!$F$7)","v":34.805827980000011},869760631542]
["BIMED","BMSC-06","M50","Káblová vývodka s metrickým závitom M50 nerezová AISI 303",15,79.104154500000007,{"$f":"F352*(1-Elteq!$F$7)","v":79.104154500000007},869760631543]
["BIMED","BMSC-07","M63","Káblová vývodka s metrickým závitom M63 nerezová AISI 303",12,94.924985400000025,{"$f":"F353*(1-Elteq!$F$7)","v":94.924985400000025},869760631544]
["BIMED","BDSM-08","M72X2","Káblová vývodka z poniklovanej mosadze M72",1,62.95627799999999,{"$f":"F354*(1-Elteq!$F$7)","v":62.95627799999999}]
["BIMED","BMBL-09","M72X2","Matica z poniklovanej mosadze pre BDSM-08",1,4.4968770000000013,{"$f":"F355*(1-Elteq!$F$7)","v":4.4968770000000013}]
["BIMED","BDSM-09S","M75X1,5","Káblová vývodka z poniklovanej mosadze M75X1,5",1,71.950032000000022,{"$f":"F356*(1-Elteq!$F$7)","v":71.950032000000022}]
["BIMED","BMBL-10S","M75X1,5","Matica z poniklovanej mosadze pre BDSM-09S",1,6.7453154999999994,{"$f":"F357*(1-Elteq!$F$7)","v":6.7453154999999994}]
["BIMED","BDSM-09","M75X2","Káblová vývodka z poniklovanej mosadze M75X2.0",1,71.950032000000022,{"$f":"F358*(1-Elteq!$F$7)","v":71.950032000000022}]
["BIMED","BMBL-10","M75X2","Matica z poniklovanej mosadze pre BDSM-09",1,6.7453154999999994,{"$f":"F359*(1-Elteq!$F$7)","v":6.7453154999999994}]
["BIMED","BDSM-10","M80X2","Káblová vývodka z poniklovanej mosadze M80X2.0 upínací rozsah 60-66",1,80.943786000000003,{"$f":"F360*(1-Elteq!$F$7)","v":80.943786000000003}]
["BIMED","BDSM-10R","M80X2","Káblová vývodka z poniklovanej mosadze M80X2.0 upínací rozsah 50-56",1,89.038164600000002,{"$f":"F361*(1-Elteq!$F$7)","v":89.038164600000002}]
["BIMED","BMBL-11","M80X2","Matica z poniklovanej mosadze pre BDSM-10/10R",1,8.9937540000000027,{"$f":"F362*(1-Elteq!$F$7)","v":8.9937540000000027}]
["BIMED","BDSM-11","M85X2","Káblová vývodka z poniklovanej mosadze M85X2.0 upínací rozsah 68-76",1,112.42192500000002,{"$f":"F363*(1-Elteq!$F$7)","v":112.42192500000002}]
["BIMED","BDSM-11R","M85X2","Káblová vývodka z poniklovanej mosadze M85X2.0 upínací rozsah 63-70",1,123.66411750000002,{"$f":"F364*(1-Elteq!$F$7)","v":123.66411750000002}]
["BIMED","BMBL-12","M85X2","Matica z poniklovanej mosadze pre BDSM-11/11R",1,11.242192500000002,{"$f":"F365*(1-Elteq!$F$7)","v":11.242192500000002}]
["BIMED","BDSM-12","M90X2","Káblová vývodka z poniklovanej mosadze M90X2.0",1,146.14850250000001,{"$f":"F366*(1-Elteq!$F$7)","v":146.14850250000001}]
["BIMED","BMBL-13","M90X2","Matica z poniklovanej mosadze pre BDSM-12",1,13.490630999999999,{"$f":"F367*(1-Elteq!$F$7)","v":13.490630999999999}]
["BIMED","BMVG-0S","M 12X1,5","Ventilačná vývodka s metrickým závitom M12X1.5 šedá","1ks",2.1621802230000005,{"$f":"F368*(1-Elteq!$F$7)","v":2.1621802230000005}]
["BIMED","BMVG-01","M 16x1,5","Ventilačná vývodka s metrickým závitom M16X1.5 šedá","1ks",2.1621802230000005,{"$f":"F369*(1-Elteq!$F$7)","v":2.1621802230000005}]
["BIMED","BMVG-02","M 20x1,5","Ventilačná vývodka s metrickým závitom M20X1.5 šedá","1ks",2.900485665000001,{"$f":"F370*(1-Elteq!$F$7)","v":2.900485665000001}]
["BIMED","BSVG-02","Pg 9","Ventilačná vývodka s PG závitom PG9 šedá","1ks",2.1621802230000005,{"$f":"F371*(1-Elteq!$F$7)","v":2.1621802230000005}]
["BIMED","BSVG-04","Pg 13,5","Ventilačná vývodka s PG závitom PG13,5 šedá","1ks",2.900485665000001,{"$f":"F372*(1-Elteq!$F$7)","v":2.900485665000001}]
["BIMED","BMVG-1S","M 12X1,5","Ventilačná vývodka s metrickým závitom M12X1.5 svetlošedá","1ks",2.1621802230000005,{"$f":"F373*(1-Elteq!$F$7)","v":2.1621802230000005}]
["BIMED","BMVG-11","M 16x1,5","Ventilačná vývodka s metrickým závitom M16X1.5 svetlošedá","1ks",2.1621802230000005,{"$f":"F374*(1-Elteq!$F$7)","v":2.1621802230000005}]
["BIMED","BMVG-12","M 20x1,5","Ventilačná vývodka s metrickým závitom M20X1.5 svetlošedá","1ks",2.900485665000001,{"$f":"F375*(1-Elteq!$F$7)","v":2.900485665000001}]
["BIMED","BSVG-12","Pg 9","Ventilačná vývodka s PG závitom PG9 svetlošedá","1ks",2.1621802230000005,{"$f":"F376*(1-Elteq!$F$7)","v":2.1621802230000005}]
["BIMED","BSVG-14","Pg 13,5","Ventilačná vývodka s PG závitom PG13,5 svetlošedá","1ks",2.900485665000001,{"$f":"F377*(1-Elteq!$F$7)","v":2.900485665000001}]
["BIMED","BMVG-2S","M 12X1,5","Ventilačná vývodka s metrickým závitom M12X1.5 čierna","1ks",2.1621802230000005,{"$f":"F378*(1-Elteq!$F$7)","v":2.1621802230000005}]
["BIMED","BMVG-21","M 16x1,5","Ventilačná vývodka s metrickým závitom M16X1.5 čierna","1ks",2.1621802230000005,{"$f":"F379*(1-Elteq!$F$7)","v":2.1621802230000005}]
["BIMED","BMVG-22","M 20x1,5","Ventilačná vývodka s metrickým závitom M20X1.5 čierna","1ks",2.900485665000001,{"$f":"F380*(1-Elteq!$F$7)","v":2.900485665000001}]
["BIMED","BSVG-22","Pg 9","Ventilačná vývodka s PG závitom PG9 čierna","1ks",2.1621802230000005,{"$f":"F381*(1-Elteq!$F$7)","v":2.1621802230000005}]
["BIMED","BSVG-24","Pg 13,5","Ventilačná vývodka s PG závitom PG13,5 čierna","1ks",2.900485665000001,{"$f":"F382*(1-Elteq!$F$7)","v":2.900485665000001}]
["BIMED","BMBCVG-0S","M 12X1,5","Ventilačná vývodka s metrickým závitom M12X1.5 ","1ks",4.7989853730000016,{"$f":"F383*(1-Elteq!$F$7)","v":4.7989853730000016}]
["BIMED","BMBCVG-01","M 16x1,5","Ventilačná vývodka s metrickým závitom M16X1.5  TL7","1ks",4.7989853730000016,{"$f":"F384*(1-Elteq!$F$7)","v":4.7989853730000016}]
["BIMED","BMBCVG-01L","M 16x1,5","Ventilačná vývodka s metrickým závitom M16X1.5  TL8","1ks",5.141770042500001,{"$f":"F385*(1-Elteq!$F$7)","v":5.141770042500001}]
["BIMED","BMBCVG-02","M 20x1,5","Ventilačná vývodka s metrickým závitom M20X1.5 ","1ks",5.9328115875000007,{"$f":"F386*(1-Elteq!$F$7)","v":5.9328115875000007}]
["BIMED","BSBCVG-01","Pg 7","Ventilačná vývodka s PG závitom PG7","1ks",4.7989853730000016,{"$f":"F387*(1-Elteq!$F$7)","v":4.7989853730000016}]
["BIMED","BSBCVG-02","Pg 9","Ventilačná vývodka s PG závitom PG9","1ks",4.7989853730000016,{"$f":"F388*(1-Elteq!$F$7)","v":4.7989853730000016}]
["BIMED","BSBCVG-03","Pg 11","Ventilačná vývodka s PG závitom PG11","1ks",4.7989853730000016,{"$f":"F389*(1-Elteq!$F$7)","v":4.7989853730000016}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"BIMED"},"BSBCVG-04","Pg 13,5","Ventilačná vývodka s PG závitom PG13.5","1ks",5.9328115875000007,{"$f":"F390*(1-Elteq!$F$7)","v":5.9328115875000007}]
["BIMED","BMOS-11","NW 16","PAT GLAND Polyamid 6 ø 16,3 ± 0,1","1ks",1.1320000000000001,{"$f":"F391*(1-Elteq!$F$7)","v":1.1320000000000001}]
["BIMED","BMOS-12","NW 20","PAT GLAND Polyamid 6 ø 20,3 ± 0,1","1ks",1.256,{"$f":"F392*(1-Elteq!$F$7)","v":1.256}]
["BIMED","BEX-16/20","NW 16/20","Špeciálny nástroj pre demontáž BMOS-11/12, BBOS-11/12","1 ks",1.256,{"$f":"F393*(1-Elteq!$F$7)","v":1.256}]
["BIMED","BMBLS-01","M12","Káblová matica s metrickým závitom M12 nerezová AISI 303",100,0.71612799999999999,{"$f":"F394*(1-Elteq!$F$7)","v":0.71612799999999999}]
["BIMED","BMBLS-02","M16","Káblová matica s metrickým závitom M16 nerezová AISI 303",100,0.77419199999999999,{"$f":"F395*(1-Elteq!$F$7)","v":0.77419199999999999}]
["BIMED","BMBLS-03","M20","Káblová matica s metrickým závitom M20 nerezová AISI 303",100,1.0645150000000001,{"$f":"F396*(1-Elteq!$F$7)","v":1.0645150000000001}]
["BIMED","BMBLS-04","M25","Káblová matica s metrickým závitom M25 nerezová AISI 303",100,1.2580629999999999,{"$f":"F397*(1-Elteq!$F$7)","v":1.2580629999999999}]
["BIMED","BMBLS-05","M32","Káblová matica s metrickým závitom M32 nerezová AISI 303",50,1.741933,{"$f":"F398*(1-Elteq!$F$7)","v":1.741933}]
["BIMED","BMBLS-06","M40","Káblová matica s metrickým závitom M40 nerezová AISI 303",50,2.3225769999999999,{"$f":"F399*(1-Elteq!$F$7)","v":2.3225769999999999}]
["BIMED","BMBLS-07","M50","Káblová matica s metrickým závitom M50 nerezová AISI 303",10,3.870962,{"$f":"F400*(1-Elteq!$F$7)","v":3.870962}]
["BIMED","BMBLS-08","M63","Káblová matica s metrickým závitom M63 nerezová AISI 303",10,5.2257990000000003,{"$f":"F401*(1-Elteq!$F$7)","v":5.2257990000000003}]
["BIMED","BMBLS-09","M72","Káblová matica s metrickým závitom M72 nerezová AISI 303",10,8.7096640000000001,{"$f":"F402*(1-Elteq!$F$7)","v":8.7096640000000001}]
["BIMED","BMBLS-10","M75","Káblová matica s metrickým závitom M75 nerezová AISI 303",5,11.03224,{"$f":"F403*(1-Elteq!$F$7)","v":11.03224}]
["BIMED","BMBLS-11","M80","Káblová matica s metrickým závitom M80 nerezová AISI 303",5,16.064489999999999,{"$f":"F404*(1-Elteq!$F$7)","v":16.064489999999999}]
["BIMED","BMBLS-12","M85","Káblová matica s metrickým závitom M85 nerezová AISI 303",5,21.290289999999999,{"$f":"F405*(1-Elteq!$F$7)","v":21.290289999999999}]
["BIMED","BMBLS-13","M90","Káblová matica s metrickým závitom M90 nerezová AISI 303",5,28.06447,{"$f":"F406*(1-Elteq!$F$7)","v":28.06447}]
["BIMED","BSLS-01","Pg7","Káblová matica s PG závitom PG7 nerezová AISI 303",100,1.683868452499502,{"$f":"F407*(1-Elteq!$F$7)","v":1.683868452499502}]
["BIMED","BSLS-02","Pg9","Káblová matica s PG závitom PG9 nerezová AISI 303",100,2.4193512248556064,{"$f":"F408*(1-Elteq!$F$7)","v":2.4193512248556064}]
["BIMED","BSLS-03","Pg11","Káblová matica s PG závitom PG11 nerezová AISI 303",100,2.7096733718382788,{"$f":"F409*(1-Elteq!$F$7)","v":2.7096733718382788}]
["BIMED","BSLS-04","Pg13,5","Káblová matica s PG závitom PG13,5 nerezová AISI 303",100,2.9999955188209517,{"$f":"F410*(1-Elteq!$F$7)","v":2.9999955188209517}]
["BIMED","BSLS-05","Pg16","Káblová matica s PG závitom PG16 nerezová AISI 303",100,3.3870917147978488,{"$f":"F411*(1-Elteq!$F$7)","v":3.3870917147978488}]
["BIMED","BSLS-06","Pg21","Káblová matica s PG závitom PG21 nerezová AISI 303",100,3.87096195976897,{"$f":"F412*(1-Elteq!$F$7)","v":3.87096195976897}]
["BIMED","BSLS-07","Pg29","Káblová matica s PG závitom PG29 nerezová AISI 303",50,4.8387024497112128,{"$f":"F413*(1-Elteq!$F$7)","v":4.8387024497112128}]
["BIMED","BSLS-08","Pg36","Káblová matica s PG závitom PG36 nerezová AISI 303",25,5.612894841665006,{"$f":"F414*(1-Elteq!$F$7)","v":5.612894841665006}]
["BIMED","BSLS-09","Pg42","Káblová matica s PG závitom PG42 nerezová AISI 303",10,6.2903131846245763,{"$f":"F415*(1-Elteq!$F$7)","v":6.2903131846245763}]
["BIMED","BSLS-10","Pg48","Káblová matica s PG závitom PG48 nerezová AISI 303",10,7.2580536745668187,{"$f":"F416*(1-Elteq!$F$7)","v":7.2580536745668187}]
["BIMED","BBOS-11","NW 16","PAT GLAND z poniklovanej mosadze ø 16,3 ± 0,1","1ks",7.2306999999999997,{"$f":"F417*(1-Elteq!$F$7)","v":7.2306999999999997}]
["BIMED","BBOS-12","NW 20","PAT GLAND z poniklovanej mosadze ø 20,3 ± 0,1","1ks",8.5871999999999993,{"$f":"F418*(1-Elteq!$F$7)","v":8.5871999999999993}]

{"sheet":"REIKU-B","index":5,"n_rows":1524,"n_cols":7,"rows_kept":1524,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["sheetname","Obj.kód čierna",null,"Popis","Balenie","Cena za ks alebo m","Cena za kus po zľave"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"AFFSS-M10",null,null,50,0.14194123564905192,{"$f":"F5*(1-Elteq!$F$8)","v":0.14194123564905192}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"AFFSS-M12",null,null,50,0.15484498434442034,{"$f":"F6*(1-Elteq!$F$8)","v":0.15484498434442034}]
["REIKU-B","AFFSS-M16",null,null,50,0.16774873303978871,{"$f":"F7*(1-Elteq!$F$8)","v":0.16774873303978871}]
["REIKU-B","AFFSS-M20",null,null,50,0.20645997912589376,{"$f":"F8*(1-Elteq!$F$8)","v":0.20645997912589376}]
["REIKU-B","AFFSS-M25",null,null,50,0.23226747651663035,{"$f":"F9*(1-Elteq!$F$8)","v":0.23226747651663035}]
["REIKU-B","AFFSS-M32",null,null,30,0.33549746607957742,{"$f":"F10*(1-Elteq!$F$8)","v":0.33549746607957742}]
["REIKU-B","AFFSS-M40",null,null,10,0.50324619911936608,{"$f":"F11*(1-Elteq!$F$8)","v":0.50324619911936608}]
["REIKU-B","AFFSS-M50",null,null,10,0.70970617824526017,{"$f":"F12*(1-Elteq!$F$8)","v":0.70970617824526017}]
["REIKU-B","AFFSS-M63",null,null,10,0.9419736547618901,{"$f":"F13*(1-Elteq!$F$8)","v":0.9419736547618901}]
["REIKU-B","AFFSS-P07",null,null,100,0.15484498434442034,{"$f":"F14*(1-Elteq!$F$8)","v":0.15484498434442034}]
["REIKU-B","AFFSS-P09",null,null,100,0.15484498434442034,{"$f":"F15*(1-Elteq!$F$8)","v":0.15484498434442034}]
["REIKU-B","AFFSS-P11",null,null,100,0.16774873303978871,{"$f":"F16*(1-Elteq!$F$8)","v":0.16774873303978871}]
["REIKU-B","AFFSS-P13",null,null,100,0.18065248173515702,{"$f":"F17*(1-Elteq!$F$8)","v":0.18065248173515702}]
["REIKU-B","AFFSS-P16",null,null,50,0.19355623043052539,{"$f":"F18*(1-Elteq!$F$8)","v":0.19355623043052539}]
["REIKU-B","AFFSS-P21",null,null,50,0.23226747651663035,{"$f":"F19*(1-Elteq!$F$8)","v":0.23226747651663035}]
["REIKU-B","AFFSS-P29",null,null,30,0.33549746607957742,{"$f":"F20*(1-Elteq!$F$8)","v":0.33549746607957742}]
["REIKU-B","AFFSS-P36",null,null,20,0.40001620955641914,{"$f":"F21*(1-Elteq!$F$8)","v":0.40001620955641914}]
["REIKU-B","AFFSS-P42",null,null,10,1.0064923982387322,{"$f":"F22*(1-Elteq!$F$8)","v":1.0064923982387322}]
["REIKU-B","AFFSS-P48",null,null,10,0.47743870172862929,{"$f":"F23*(1-Elteq!$F$8)","v":0.47743870172862929}]
["REIKU-B","BIORRB-12F",null,null,50,2.1108113631497707,{"$f":"F24*(1-Elteq!$F$8)","v":2.1108113631497707}]
["REIKU-B","BIORRB-17F",null,null,50,3.220214544712209,{"$f":"F25*(1-Elteq!$F$8)","v":3.220214544712209}]
["REIKU-B","BIORRB-23F",null,null,50,5.134671362452699,{"$f":"F26*(1-Elteq!$F$8)","v":5.134671362452699}]
["REIKU-B","BIORRB-29F",null,null,50,6.5091531803176652,{"$f":"F27*(1-Elteq!$F$8)","v":6.5091531803176652}]
["REIKU-B","BIORRB-36G",null,null,30,9.2679345433180647,{"$f":"F28*(1-Elteq!$F$8)","v":9.2679345433180647}]
["REIKU-B","BIORRB-48G",null,null,30,12.821951815226052,{"$f":"F29*(1-Elteq!$F$8)","v":12.821951815226052}]
["REIKU-B","BIORRB-52G",null,null,"10/30",18.358364577586137,{"$f":"F30*(1-Elteq!$F$8)","v":18.358364577586137}]
["REIKU-B","BIORRB-70G",null,null,"10/30",30.376048174815772,{"$f":"F31*(1-Elteq!$F$8)","v":30.376048174815772}]
["REIKU-B","EMV M16",null,null,30,21.949276530821589,{"$f":"F32*(1-Elteq!$F$8)","v":21.949276530821589}]
["REIKU-B","EMV M20",null,null,20,23.755801348173158,{"$f":"F33*(1-Elteq!$F$8)","v":23.755801348173158}]
["REIKU-B","EMV M25",null,null,20,26.233321097683874,{"$f":"F34*(1-Elteq!$F$8)","v":26.233321097683874}]
["REIKU-B","EMV M32",null,null,10,32.67229169667268,{"$f":"F35*(1-Elteq!$F$8)","v":32.67229169667268}]
["REIKU-B","EMV M40",null,null,10,39.575797248694748,{"$f":"F36*(1-Elteq!$F$8)","v":39.575797248694748}]
["REIKU-B","EMV M50",null,null,10,53.215059619699105,{"$f":"F37*(1-Elteq!$F$8)","v":53.215059619699105}]
["REIKU-B","EMV M63",null,null,10,56.440996793541203,{"$f":"F38*(1-Elteq!$F$8)","v":56.440996793541203}]
["REIKU-B","EMV P16",null,null,30,21.949276530821589,{"$f":"F39*(1-Elteq!$F$8)","v":21.949276530821589}]
["REIKU-B","EMV P21",null,null,20,23.755801348173158,{"$f":"F40*(1-Elteq!$F$8)","v":23.755801348173158}]
["REIKU-B","EMV P29",null,null,20,26.233321097683874,{"$f":"F41*(1-Elteq!$F$8)","v":26.233321097683874}]
["REIKU-B","EMV P36",null,null,10,32.67229169667268,{"$f":"F42*(1-Elteq!$F$8)","v":32.67229169667268}]
["REIKU-B","EMV P48",null,null,10,39.575797248694748,{"$f":"F43*(1-Elteq!$F$8)","v":39.575797248694748}]
["REIKU-B","FSSF-23-600",null,null,1,74.331976710137425,{"$f":"F44*(1-Elteq!$F$8)","v":74.331976710137425}]
["REIKU-B","FSSF-29-400",null,null,1,57.341810604963172,{"$f":"F45*(1-Elteq!$F$8)","v":57.341810604963172}]
["REIKU-B","FSSF-36-400",null,null,1,57.341810604963143,{"$f":"F46*(1-Elteq!$F$8)","v":57.341810604963143}]
["REIKU-B","FSMF-29-600",null,null,1,74.331976710137425,{"$f":"F47*(1-Elteq!$F$8)","v":74.331976710137425}]
["REIKU-B","FSMF-36-400",null,null,1,67.960664420697086,{"$f":"F48*(1-Elteq!$F$8)","v":67.960664420697086}]
["REIKU-B","FSMF-36-600",null,null,1,82.827059762724573,{"$f":"F49*(1-Elteq!$F$8)","v":82.827059762724573}]
["REIKU-B","FSMF-48-550",null,null,1,108.48588633862778,{"$f":"F50*(1-Elteq!$F$8)","v":108.48588633862778}]
["REIKU-B","FSMF-52-1000",null,null,1,106.1885381573392,{"$f":"F51*(1-Elteq!$F$8)","v":106.1885381573392}]
["REIKU-B","FSMF-52-52-1000",null,null,1,163.36698178052188,{"$f":"F52*(1-Elteq!$F$8)","v":163.36698178052188}]
["REIKU-B","FSMF-70-550",null,null,1,63.713122894403497,{"$f":"F53*(1-Elteq!$F$8)","v":63.713122894403497}]
["REIKU-B","FSMF-70-1000",null,null,1,104.06476739419239,{"$f":"F54*(1-Elteq!$F$8)","v":104.06476739419239}]
["REIKU-B","FSVF-52-1000",null,null,1,106.1885381573392,{"$f":"F55*(1-Elteq!$F$8)","v":106.1885381573392}]
["REIKU-B","FSVF-70-1000",null,null,1,116.80739197307312,{"$f":"F56*(1-Elteq!$F$8)","v":116.80739197307312}]
["REIKU-B","LPRRB-10F",null,null,100,1.5822537964926726,{"$f":"F57*(1-Elteq!$F$8)","v":1.5822537964926726}]
["REIKU-B","LPRRB-12F",null,null,50,2.1684235743846361,{"$f":"F58*(1-Elteq!$F$8)","v":2.1684235743846361}]
["REIKU-B","LPRRB-17F",null,null,50,3.3756602092665307,{"$f":"F59*(1-Elteq!$F$8)","v":3.3756602092665307}]
["REIKU-B","LPRRB-23G",null,null,50,5.321298807670658,{"$f":"F60*(1-Elteq!$F$8)","v":5.321298807670658}]
["REIKU-B","LPRRB-29G",null,null,50,6.7394351814489708,{"$f":"F61*(1-Elteq!$F$8)","v":6.7394351814489708}]
["REIKU-B","LPRRB-36G",null,null,30,9.5759608063903681,{"$f":"F62*(1-Elteq!$F$8)","v":9.5759608063903681}]
["REIKU-B","LPRRB-48G",null,null,30,13.830622805110076,{"$f":"F63*(1-Elteq!$F$8)","v":13.830622805110076}]
["REIKU-B","LPRRB-52G",null,null,"10/30",20.077958595800737,{"$f":"F64*(1-Elteq!$F$8)","v":20.077958595800737}]
["REIKU-B","LPRRB-70G",null,null,"10/30",32.689459528944809,{"$f":"F65*(1-Elteq!$F$8)","v":32.689459528944809}]
["REIKU-B","LPRRB-95G",null,null,"10/30",44.159940908001886,{"$f":"F66*(1-Elteq!$F$8)","v":44.159940908001886}]
["REIKU-B","MES1B-07",null,null,100,0.45163120433789261,{"$f":"F67*(1-Elteq!$F$8)","v":0.45163120433789261}]
["REIKU-B","MES1B-10",null,null,100,0.4645349530332607,{"$f":"F68*(1-Elteq!$F$8)","v":0.4645349530332607}]
["REIKU-B","MES1B-12",null,null,100,0.47743870172862929,{"$f":"F69*(1-Elteq!$F$8)","v":0.47743870172862929}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"MES1B-14",null,null,100,0.54186312005079662,{"$f":"F70*(1-Elteq!$F$8)","v":0.54186312005079662}]
["REIKU-B","MES1B-17",null,null,100,0.54195744520547118,{"$f":"F71*(1-Elteq!$F$8)","v":0.54195744520547118}]
["REIKU-B","MES1B-23",null,null,50,0.58066869129157628,{"$f":"F72*(1-Elteq!$F$8)","v":0.58066869129157628}]
["REIKU-B","MES1B-29",null,null,30,0.67099493215915484,{"$f":"F73*(1-Elteq!$F$8)","v":0.67099493215915484}]
["REIKU-B","MES1B-36",null,null,20,0.78712867041746981,{"$f":"F74*(1-Elteq!$F$8)","v":0.78712867041746981}]
["REIKU-B","MES1B-48",null,null,20,1.1484336338877841,{"$f":"F75*(1-Elteq!$F$8)","v":1.1484336338877841}]
["REIKU-B","MES1B-52",null,null,20,1.6645835817025187,{"$f":"F76*(1-Elteq!$F$8)","v":1.6645835817025187}]
["REIKU-B","MES1B-70",null,null,10,2.6065572364644094,{"$f":"F77*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-B","MES2B-52",null,null,20,1.4710273512719934,{"$f":"F78*(1-Elteq!$F$8)","v":1.4710273512719934}]
["REIKU-B","MES2B-70",null,null,10,2.6065572364644094,{"$f":"F79*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-B","MES2B-95",null,null,10,3.5743383886170359,{"$f":"F80*(1-Elteq!$F$8)","v":3.5743383886170359}]
["REIKU-B","MSGMM-M12",null,null,100,0.4645349530332607,{"$f":"F81*(1-Elteq!$F$8)","v":0.4645349530332607}]
["REIKU-B","MSGMM-M16",null,null,100,0.49034245042399766,{"$f":"F82*(1-Elteq!$F$8)","v":0.49034245042399766}]
["REIKU-B","MSGMM-M20",null,null,100,0.50324619911936608,{"$f":"F83*(1-Elteq!$F$8)","v":0.50324619911936608}]
["REIKU-B","MSGMM-M25",null,null,100,0.70970617824526017,{"$f":"F84*(1-Elteq!$F$8)","v":0.70970617824526017}]
["REIKU-B","MSGMM-M32",null,null,50,0.99358864954336401,{"$f":"F85*(1-Elteq!$F$8)","v":0.99358864954336401}]
["REIKU-B","MSGMM-M40",null,null,25,1.6774873303978866,{"$f":"F86*(1-Elteq!$F$8)","v":1.6774873303978866}]
["REIKU-B","MSGMM-M50",null,null,25,3.9098358546966128,{"$f":"F87*(1-Elteq!$F$8)","v":3.9098358546966128}]
["REIKU-B","MSGMM-M63",null,null,25,5.0840769859751331,{"$f":"F88*(1-Elteq!$F$8)","v":5.0840769859751331}]
["REIKU-B","MSGMM-P07",null,null,100,0.15484498434442034,{"$f":"F89*(1-Elteq!$F$8)","v":0.15484498434442034}]
["REIKU-B","MSGMM-P09",null,null,100,0.15484498434442034,{"$f":"F90*(1-Elteq!$F$8)","v":0.15484498434442034}]
["REIKU-B","MSGMM-P11",null,null,100,0.16774873303978871,{"$f":"F91*(1-Elteq!$F$8)","v":0.16774873303978871}]
["REIKU-B","MSGMM-P13",null,null,100,0.18065248173515702,{"$f":"F92*(1-Elteq!$F$8)","v":0.18065248173515702}]
["REIKU-B","MSGMM-P16",null,null,100,0.24517122521199883,{"$f":"F93*(1-Elteq!$F$8)","v":0.24517122521199883}]
["REIKU-B","MSGMM-P21",null,null,100,0.30968996868884069,{"$f":"F94*(1-Elteq!$F$8)","v":0.30968996868884069}]
["REIKU-B","MSGMM-P29",null,null,100,0.47743870172862929,{"$f":"F95*(1-Elteq!$F$8)","v":0.47743870172862929}]
["REIKU-B","MSGMM-P36",null,null,50,0.85164741389431153,{"$f":"F96*(1-Elteq!$F$8)","v":0.85164741389431153}]
["REIKU-B","MSGMM-P48",null,null,50,1.7936210686562022,{"$f":"F97*(1-Elteq!$F$8)","v":1.7936210686562022}]
["REIKU-B","MSGRM-10M16 /price upon enquiry/",null,null,null,null,{"$f":"F98*(1-Elteq!$F$8)","v":0}]
["REIKU-B","MSGRM-12M20 /price upon enquiry/",null,null,null,null,{"$f":"F99*(1-Elteq!$F$8)","v":0}]
["REIKU-B","MSGRM-17M25 /price upon enquiry/",null,null,null,null,{"$f":"F100*(1-Elteq!$F$8)","v":0}]
["REIKU-B","MSGRM-23M32 /price upon enquiry/",null,null,null,null,{"$f":"F101*(1-Elteq!$F$8)","v":0}]
["REIKU-B","MSGRM-29M40 /price upon enquiry/",null,null,null,null,{"$f":"F102*(1-Elteq!$F$8)","v":0}]
["REIKU-B","MSGRM-36M50 /price upon enquiry/",null,null,null,null,{"$f":"F103*(1-Elteq!$F$8)","v":0}]
["REIKU-B","MSGRM-48M63 /price upon enquiry/",null,null,null,null,{"$f":"F104*(1-Elteq!$F$8)","v":0}]
["REIKU-B","MSGVM-10M16 /price upon enquiry/",null,null,null,null,{"$f":"F105*(1-Elteq!$F$8)","v":0}]
["REIKU-B","MSGVM-12M20 /price upon enquiry/",null,null,null,null,{"$f":"F106*(1-Elteq!$F$8)","v":0}]
["REIKU-B","MSGVM-17M25 /price upon enquiry/",null,null,null,null,{"$f":"F107*(1-Elteq!$F$8)","v":0}]
["REIKU-B","MSGVM-23M32 /price upon enquiry/",null,null,null,null,{"$f":"F108*(1-Elteq!$F$8)","v":0}]
["REIKU-B","MSGVM-29M40 /price upon enquiry/",null,null,null,null,{"$f":"F109*(1-Elteq!$F$8)","v":0}]
["REIKU-B","MSGVM-36M50 /price upon enquiry/",null,null,null,null,{"$f":"F110*(1-Elteq!$F$8)","v":0}]
["REIKU-B","MSGVM-48M63 /price upon enquiry/",null,null,null,null,{"$f":"F111*(1-Elteq!$F$8)","v":0}]
["REIKU-B","MSKOM-M12",null,null,50,2.0516960425635697,{"$f":"F112*(1-Elteq!$F$8)","v":2.0516960425635697}]
["REIKU-B","MSKOM-M16",null,null,50,4.0517770903456647,{"$f":"F113*(1-Elteq!$F$8)","v":4.0517770903456647}]
["REIKU-B","MSKOM-M20",null,null,50,5.6002269337898714,{"$f":"F114*(1-Elteq!$F$8)","v":5.6002269337898714}]
["REIKU-B","MSKOM-M25",null,null,50,5.3937669546639748,{"$f":"F115*(1-Elteq!$F$8)","v":5.3937669546639748}]
["REIKU-B","MSKOM-M32",null,null,25,8.7229341180690128,{"$f":"F116*(1-Elteq!$F$8)","v":8.7229341180690128}]
["REIKU-B","MSKOM-M40",null,null,10,16.078070874428974,{"$f":"F117*(1-Elteq!$F$8)","v":16.078070874428974}]
["REIKU-B","MSKOM-M50",null,null,5,31.536761811480272,{"$f":"F118*(1-Elteq!$F$8)","v":31.536761811480272}]
["REIKU-B","MSKOM-M63",null,null,5,31.975489267122796,{"$f":"F119*(1-Elteq!$F$8)","v":31.975489267122796}]
["REIKU-B","MSKOM-P07",null,null,50,1.8065248173515704,{"$f":"F120*(1-Elteq!$F$8)","v":1.8065248173515704}]
["REIKU-B","MSKOM-P09",null,null,50,2.1420222834311482,{"$f":"F121*(1-Elteq!$F$8)","v":2.1420222834311482}]
["REIKU-B","MSKOM-P11",null,null,50,2.5420384929875666,{"$f":"F122*(1-Elteq!$F$8)","v":2.5420384929875666}]
["REIKU-B","MSKOM-P13",null,null,50,2.8259209642856709,{"$f":"F123*(1-Elteq!$F$8)","v":2.8259209642856709}]
["REIKU-B","MSKOM-P16",null,null,50,3.2646484199281942,{"$f":"F124*(1-Elteq!$F$8)","v":3.2646484199281942}]
["REIKU-B","MSKOM-P21",null,null,50,5.3808632059686072,{"$f":"F125*(1-Elteq!$F$8)","v":5.3808632059686072}]
["REIKU-B","MSKOM-P29",null,null,25,8.6971266206782758,{"$f":"F126*(1-Elteq!$F$8)","v":8.6971266206782758}]
["REIKU-B","MSKOM-P36",null,null,10,16.013552130952135,{"$f":"F127*(1-Elteq!$F$8)","v":16.013552130952135}]
["REIKU-B","MSKOM-P48",null,null,5,38.143481143508879,{"$f":"F128*(1-Elteq!$F$8)","v":38.143481143508879}]
["REIKU-B","MSM 1216",null,null,50,0.99358864954336401,{"$f":"F129*(1-Elteq!$F$8)","v":0.99358864954336401}]
["REIKU-B","MSM 1612",null,null,50,0.77422492172210156,{"$f":"F130*(1-Elteq!$F$8)","v":0.77422492172210156}]
["REIKU-B","MSM 1620",null,null,50,1.3290861156229412,{"$f":"F131*(1-Elteq!$F$8)","v":1.3290861156229412}]
["REIKU-B","MSM 2012",null,null,50,1.0839148904109424,{"$f":"F132*(1-Elteq!$F$8)","v":1.0839148904109424}]
["REIKU-B","MSM 2016",null,null,50,1.0839148904109424,{"$f":"F133*(1-Elteq!$F$8)","v":1.0839148904109424}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"MSM 2025",null,null,50,2.2323485242987262,{"$f":"F134*(1-Elteq!$F$8)","v":2.2323485242987262}]
["REIKU-B","MSM 2516",null,null,50,2.1033110373450428,{"$f":"F135*(1-Elteq!$F$8)","v":2.1033110373450428}]
["REIKU-B","MSM 2520",null,null,50,1.780717319960833,{"$f":"F136*(1-Elteq!$F$8)","v":1.780717319960833}]
["REIKU-B","MSM 2532",null,null,25,2.8130172155903033,{"$f":"F137*(1-Elteq!$F$8)","v":2.8130172155903033}]
["REIKU-B","MSM 3220",null,null,50,3.1485146816698792,{"$f":"F138*(1-Elteq!$F$8)","v":3.1485146816698792}]
["REIKU-B","MSM 3225",null,null,50,3.0012556640354111,{"$f":"F139*(1-Elteq!$F$8)","v":3.0012556640354111}]
["REIKU-B","MSM 3240",null,null,25,4.425985802511347,{"$f":"F140*(1-Elteq!$F$8)","v":4.425985802511347}]
["REIKU-B","MSM 4025",null,null,25,5.109884483365871,{"$f":"F141*(1-Elteq!$F$8)","v":5.109884483365871}]
["REIKU-B","MSM 4032",null,null,25,4.1937183259947179,{"$f":"F142*(1-Elteq!$F$8)","v":4.1937183259947179}]
["REIKU-B","MSM 4050",null,null,10,7.0067355415850194,{"$f":"F143*(1-Elteq!$F$8)","v":7.0067355415850194}]
["REIKU-B","MSM 5032",null,null,25,7.0067355415850194,{"$f":"F144*(1-Elteq!$F$8)","v":7.0067355415850194}]
["REIKU-B","MSM 5040",null,null,25,5.6776494259620813,{"$f":"F145*(1-Elteq!$F$8)","v":5.6776494259620813}]
["REIKU-B","MSM 5063",null,null,10,16.942622037018655,{"$f":"F146*(1-Elteq!$F$8)","v":16.942622037018655}]
["REIKU-B","MSM 6340",null,null,10,12.865037449282251,{"$f":"F147*(1-Elteq!$F$8)","v":12.865037449282251}]
["REIKU-B","MSM 6350",null,null,10,11.62627757452689,{"$f":"F148*(1-Elteq!$F$8)","v":11.62627757452689}]
["REIKU-B","MSP0709",null,null,100,0.73551367563599668,{"$f":"F149*(1-Elteq!$F$8)","v":0.73551367563599668}]
["REIKU-B","MSP0907",null,null,100,0.43872745564252419,{"$f":"F150*(1-Elteq!$F$8)","v":0.43872745564252419}]
["REIKU-B","MSP0911",null,null,100,0.58066869129157628,{"$f":"F151*(1-Elteq!$F$8)","v":0.58066869129157628}]
["REIKU-B","MSP0913",null,null,100,1.0968186391063106,{"$f":"F152*(1-Elteq!$F$8)","v":1.0968186391063106}]
["REIKU-B","MSP1107",null,null,100,0.65809118346378659,{"$f":"F153*(1-Elteq!$F$8)","v":0.65809118346378659}]
["REIKU-B","MSP1109",null,null,100,0.58066869129157628,{"$f":"F154*(1-Elteq!$F$8)","v":0.58066869129157628}]
["REIKU-B","MSP1113",null,null,100,1.0322998956294691,{"$f":"F155*(1-Elteq!$F$8)","v":1.0322998956294691}]
["REIKU-B","MSP1116",null,null,100,1.1871448799738891,{"$f":"F156*(1-Elteq!$F$8)","v":1.1871448799738891}]
["REIKU-B","MSP1121",null,null,100,2.0516960425635697,{"$f":"F157*(1-Elteq!$F$8)","v":2.0516960425635697}]
["REIKU-B","MSP1307",null,null,100,0.63228368607304952,{"$f":"F158*(1-Elteq!$F$8)","v":0.63228368607304952}]
["REIKU-B","MSP1309",null,null,100,0.55486119390083954,{"$f":"F159*(1-Elteq!$F$8)","v":0.55486119390083954}]
["REIKU-B","MSP1311",null,null,100,0.45163120433789261,{"$f":"F160*(1-Elteq!$F$8)","v":0.45163120433789261}]
["REIKU-B","MSP1316",null,null,100,0.73551367563599668,{"$f":"F161*(1-Elteq!$F$8)","v":0.73551367563599668}]
["REIKU-B","MSP1321",null,null,100,1.638776084311782,{"$f":"F162*(1-Elteq!$F$8)","v":1.638776084311782}]
["REIKU-B","MSP1607",null,null,100,0.9290699060665214,{"$f":"F163*(1-Elteq!$F$8)","v":0.9290699060665214}]
["REIKU-B","MSP1609",null,null,100,0.86455116258968001,{"$f":"F164*(1-Elteq!$F$8)","v":0.86455116258968001}]
["REIKU-B","MSP1611",null,null,100,0.51614994781473456,{"$f":"F165*(1-Elteq!$F$8)","v":0.51614994781473456}]
["REIKU-B","MSP1613",null,null,100,0.45163120433789261,{"$f":"F166*(1-Elteq!$F$8)","v":0.45163120433789261}]
["REIKU-B","MSP1621",null,null,50,1.8452360634376752,{"$f":"F167*(1-Elteq!$F$8)","v":1.8452360634376752}]
["REIKU-B","MSP1629",null,null,50,4.3356595616437694,{"$f":"F168*(1-Elteq!$F$8)","v":4.3356595616437694}]
["REIKU-B","MSP2111",null,null,100,1.65167983300715,{"$f":"F169*(1-Elteq!$F$8)","v":1.65167983300715}]
["REIKU-B","MSP2113",null,null,100,1.8065248173515704,{"$f":"F170*(1-Elteq!$F$8)","v":1.8065248173515704}]
["REIKU-B","MSP2116",null,null,100,0.85164741389431153,{"$f":"F171*(1-Elteq!$F$8)","v":0.85164741389431153}]
["REIKU-B","MSP2129",null,null,50,3.2259371738420892,{"$f":"F172*(1-Elteq!$F$8)","v":3.2259371738420892}]
["REIKU-B","MSP2916",null,null,50,2.0000810477820958,{"$f":"F173*(1-Elteq!$F$8)","v":2.0000810477820958}]
["REIKU-B","MSP2921",null,null,50,1.9484660530006226,{"$f":"F174*(1-Elteq!$F$8)","v":1.9484660530006226}]
["REIKU-B","MSP2936",null,null,25,3.6517608807892468,{"$f":"F175*(1-Elteq!$F$8)","v":3.6517608807892468}]
["REIKU-B","MSP3621",null,null,25,4.8518095094585032,{"$f":"F176*(1-Elteq!$F$8)","v":4.8518095094585032}]
["REIKU-B","MSP3629",null,null,25,2.5678459903783031,{"$f":"F177*(1-Elteq!$F$8)","v":2.5678459903783031}]
["REIKU-B","MSP4229",null,null,25,14.916733491845822,{"$f":"F178*(1-Elteq!$F$8)","v":14.916733491845822}]
["REIKU-B","MSP4236",null,null,25,3.1872259277559856,{"$f":"F179*(1-Elteq!$F$8)","v":3.1872259277559856}]
["REIKU-B","MSP4248",null,null,25,11.406913846705633,{"$f":"F180*(1-Elteq!$F$8)","v":11.406913846705633}]
["REIKU-B","MSP4836",null,null,25,10.542362684115947,{"$f":"F181*(1-Elteq!$F$8)","v":10.542362684115947}]
["REIKU-B","MSP4842",null,null,25,7.4583667459229108,{"$f":"F182*(1-Elteq!$F$8)","v":7.4583667459229108}]
["REIKU-B","MSPAM-M16",null,null,50,1.72910232517936,{"$f":"F183*(1-Elteq!$F$8)","v":1.72910232517936}]
["REIKU-B","MSPAM-M20",null,null,50,1.8194285660469385,{"$f":"F184*(1-Elteq!$F$8)","v":1.8194285660469385}]
["REIKU-B","MSPAM-M25",null,null,50,2.8001134668949357,{"$f":"F185*(1-Elteq!$F$8)","v":2.8001134668949357}]
["REIKU-B","MSPAM-M32",null,null,25,3.4065896555772461,{"$f":"F186*(1-Elteq!$F$8)","v":3.4065896555772461}]
["REIKU-B","MSPAM-M40",null,null,25,4.2711408181669279,{"$f":"F187*(1-Elteq!$F$8)","v":4.2711408181669279}]
["REIKU-B","MSPAM-M50",null,null,25,4.8706898485330443,{"$f":"F188*(1-Elteq!$F$8)","v":4.8706898485330443}]
["REIKU-B","MSPAM-M63",null,null,25,11.291328837718238,{"$f":"F189*(1-Elteq!$F$8)","v":11.291328837718238}]
["REIKU-B","MSPAM-P09",null,null,50,1.72910232517936,{"$f":"F190*(1-Elteq!$F$8)","v":1.72910232517936}]
["REIKU-B","MSPAM-P11",null,null,50,1.72910232517936,{"$f":"F191*(1-Elteq!$F$8)","v":1.72910232517936}]
["REIKU-B","MSPAM-P16",null,null,50,1.8194285660469385,{"$f":"F192*(1-Elteq!$F$8)","v":1.8194285660469385}]
["REIKU-B","MSPAM-P21",null,null,50,2.8001134668949357,{"$f":"F193*(1-Elteq!$F$8)","v":2.8001134668949357}]
["REIKU-B","MSPAM-P29",null,null,50,3.4065896555772461,{"$f":"F194*(1-Elteq!$F$8)","v":3.4065896555772461}]
["REIKU-B","MSPAM-P36",null,null,25,4.2711408181669279,{"$f":"F195*(1-Elteq!$F$8)","v":4.2711408181669279}]
["REIKU-B","MSPAM-P42",null,null,25,11.01980138584458,{"$f":"F196*(1-Elteq!$F$8)","v":11.01980138584458}]
["REIKU-B","MSPAM-P48",null,null,25,14.400583544031091,{"$f":"F197*(1-Elteq!$F$8)","v":14.400583544031091}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"NIDRB-17",null,null,30,0.40001620955641914,{"$f":"F198*(1-Elteq!$F$8)","v":0.40001620955641914}]
["REIKU-B","NIDRB-23",null,null,30,0.49034245042399766,{"$f":"F199*(1-Elteq!$F$8)","v":0.49034245042399766}]
["REIKU-B","NIDRB-29",null,null,20,0.65809118346378659,{"$f":"F200*(1-Elteq!$F$8)","v":0.65809118346378659}]
["REIKU-B","NIDRB-36",null,null,10,0.91616615737115359,{"$f":"F201*(1-Elteq!$F$8)","v":0.91616615737115359}]
["REIKU-B","NIDRB-48",null,null,10,1.264567372146099,{"$f":"F202*(1-Elteq!$F$8)","v":1.264567372146099}]
["REIKU-B","NIFSB-52",null,null,10,1.3032600971541126,{"$f":"F203*(1-Elteq!$F$8)","v":1.3032600971541126}]
["REIKU-B","NIFSB-70",null,null,10,1.3032786182322047,{"$f":"F204*(1-Elteq!$F$8)","v":1.3032786182322047}]
["REIKU-B","NIFSB-95",null,null,10,1.3032786182322047,{"$f":"F205*(1-Elteq!$F$8)","v":1.3032786182322047}]
["REIKU-B","PAABB-12F",null,null,50,6.0673554531467824,{"$f":"F206*(1-Elteq!$F$8)","v":6.0673554531467824}]
["REIKU-B","PAABB-17F",null,null,50,9.4348359069159518,{"$f":"F207*(1-Elteq!$F$8)","v":9.4348359069159518}]
["REIKU-B","PAABB-23F",null,null,50,14.883674542023503,{"$f":"F208*(1-Elteq!$F$8)","v":14.883674542023503}]
["REIKU-B","PAABB-29F",null,null,50,18.859854086561445,{"$f":"F209*(1-Elteq!$F$8)","v":18.859854086561445}]
["REIKU-B","PAABB-36G",null,null,30,27.270504684622587,{"$f":"F210*(1-Elteq!$F$8)","v":27.270504684622587}]
["REIKU-B","PAABB-48G",null,null,30,38.425210054778432,{"$f":"F211*(1-Elteq!$F$8)","v":38.425210054778432}]
["REIKU-B","PAAOB-07M101",null,null,50,2.3912867506472817,{"$f":"F212*(1-Elteq!$F$8)","v":2.3912867506472817}]
["REIKU-B","PAAOB-07M16",null,null,50,2.3912867506472817,{"$f":"F213*(1-Elteq!$F$8)","v":2.3912867506472817}]
["REIKU-B","PAAOB-07M20",null,null,50,2.3912867506472817,{"$f":"F214*(1-Elteq!$F$8)","v":2.3912867506472817}]
["REIKU-B","PAAOB-07P07",null,null,50,2.4259047547292516,{"$f":"F215*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-B","PAAOB-07P09",null,null,50,2.4259047547292516,{"$f":"F216*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-B","PAAOB-07P11",null,null,50,2.3912867506472817,{"$f":"F217*(1-Elteq!$F$8)","v":2.3912867506472817}]
["REIKU-B","PAAOB-07P13",null,null,50,2.3912867506472817,{"$f":"F218*(1-Elteq!$F$8)","v":2.3912867506472817}]
["REIKU-B","PAAOB-07P16",null,null,50,2.3912867506472817,{"$f":"F219*(1-Elteq!$F$8)","v":2.3912867506472817}]
["REIKU-B","PAAOB-10P09",null,null,50,2.4259047547292516,{"$f":"F220*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-B","PAAOB-12P11",null,null,50,2.4775197495107255,{"$f":"F221*(1-Elteq!$F$8)","v":2.4775197495107255}]
["REIKU-B","PAAOB-17P16",null,null,50,2.6065572364644094,{"$f":"F222*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-B","PAAOB-23P21",null,null,30,4.2969483155576649,{"$f":"F223*(1-Elteq!$F$8)","v":4.2969483155576649}]
["REIKU-B","PAAOB-29P29",null,null,30,6.2583181172536539,{"$f":"F224*(1-Elteq!$F$8)","v":6.2583181172536539}]
["REIKU-B","PAAVB-07P07",null,null,50,2.7614022208088285,{"$f":"F225*(1-Elteq!$F$8)","v":2.7614022208088285}]
["REIKU-B","PAAVB-07P09",null,null,50,2.7614022208088285,{"$f":"F226*(1-Elteq!$F$8)","v":2.7614022208088285}]
["REIKU-B","PAAVB-10P09",null,null,50,2.7743059695041974,{"$f":"F227*(1-Elteq!$F$8)","v":2.7743059695041974}]
["REIKU-B","PAAVB-12P11",null,null,50,2.8517284616764083,{"$f":"F228*(1-Elteq!$F$8)","v":2.8517284616764083}]
["REIKU-B","PAAVB-17P16",null,null,50,3.0323809434115661,{"$f":"F229*(1-Elteq!$F$8)","v":3.0323809434115661}]
["REIKU-B","PAAVB-23P21",null,null,30,4.9421357503260825,{"$f":"F230*(1-Elteq!$F$8)","v":4.9421357503260825}]
["REIKU-B","PAAVB-29P29",null,null,30,7.0970617824525961,{"$f":"F231*(1-Elteq!$F$8)","v":7.0970617824525961}]
["REIKU-B","PABSG-M12",null,null,100,0.14194123564905192,{"$f":"F232*(1-Elteq!$F$8)","v":0.14194123564905192}]
["REIKU-B","PABSG-M16",null,null,100,0.14194123564905192,{"$f":"F233*(1-Elteq!$F$8)","v":0.14194123564905192}]
["REIKU-B","PABSG-M20",null,null,100,0.16774873303978871,{"$f":"F234*(1-Elteq!$F$8)","v":0.16774873303978871}]
["REIKU-B","PABSG-M25",null,null,50,0.20645997912589376,{"$f":"F235*(1-Elteq!$F$8)","v":0.20645997912589376}]
["REIKU-B","PABSG-M32",null,null,50,0.36130496347031404,{"$f":"F236*(1-Elteq!$F$8)","v":0.36130496347031404}]
["REIKU-B","PABSG-M40",null,null,25,1.65167983300715,{"$f":"F237*(1-Elteq!$F$8)","v":1.65167983300715}]
["REIKU-B","PABSG-M50",null,null,25,2.2323485242987262,{"$f":"F238*(1-Elteq!$F$8)","v":2.2323485242987262}]
["REIKU-B","PABSG-M63",null,null,25,2.9549584512393556,{"$f":"F239*(1-Elteq!$F$8)","v":2.9549584512393556}]
["REIKU-B","PABSG-P07",null,null,100,0.14194123564905192,{"$f":"F240*(1-Elteq!$F$8)","v":0.14194123564905192}]
["REIKU-B","PABSG-P09",null,null,100,0.15484498434442034,{"$f":"F241*(1-Elteq!$F$8)","v":0.15484498434442034}]
["REIKU-B","PABSG-P11",null,null,100,0.15484498434442034,{"$f":"F242*(1-Elteq!$F$8)","v":0.15484498434442034}]
["REIKU-B","PABSG-P13",null,null,100,0.18065248173515702,{"$f":"F243*(1-Elteq!$F$8)","v":0.18065248173515702}]
["REIKU-B","PABSG-P16",null,null,100,0.19355623043052539,{"$f":"F244*(1-Elteq!$F$8)","v":0.19355623043052539}]
["REIKU-B","PABSG-P21",null,null,100,0.23226747651663035,{"$f":"F245*(1-Elteq!$F$8)","v":0.23226747651663035}]
["REIKU-B","PABSG-P29",null,null,50,0.50324619911936608,{"$f":"F246*(1-Elteq!$F$8)","v":0.50324619911936608}]
["REIKU-B","PABSG-P36",null,null,25,1.1097223878016791,{"$f":"F247*(1-Elteq!$F$8)","v":1.1097223878016791}]
["REIKU-B","PABSG-P48",null,null,25,1.5613535921395714,{"$f":"F248*(1-Elteq!$F$8)","v":1.5613535921395714}]
["REIKU-B","PACSB",null,null,50,0.23226747651663035,{"$f":"F249*(1-Elteq!$F$8)","v":0.23226747651663035}]
["REIKU-B","PADFB-42",null,null,10,9.6115549977843049,{"$f":"F250*(1-Elteq!$F$8)","v":9.6115549977843049}]
["REIKU-B","PADFB-52",null,null,10,12.452117491030469,{"$f":"F251*(1-Elteq!$F$8)","v":12.452117491030469}]
["REIKU-B","PADFB-70",null,null,10,13.677973617090462,{"$f":"F252*(1-Elteq!$F$8)","v":13.677973617090462}]
["REIKU-B","PADGB-70",null,null,10,7.2260992694062818,{"$f":"F253*(1-Elteq!$F$8)","v":7.2260992694062818}]
["REIKU-B","PADMB-70",null,null,10,11.09722387801679,{"$f":"F254*(1-Elteq!$F$8)","v":11.09722387801679}]
["REIKU-B","PADPB-36G",null,null,10,7.1374877256273646,{"$f":"F255*(1-Elteq!$F$8)","v":7.1374877256273646}]
["REIKU-B","PADPB-52",null,null,10,7.7305255778542916,{"$f":"F256*(1-Elteq!$F$8)","v":7.7305255778542916}]
["REIKU-B","PADPB-68",null,null,10,11.503823751893545,{"$f":"F257*(1-Elteq!$F$8)","v":11.503823751893545}]
["REIKU-B","PADPB-70",null,null,10,11.503813695399153,{"$f":"F258*(1-Elteq!$F$8)","v":11.503813695399153}]
["REIKU-B","PADSB-07/10",null,null,100,0.24517122521199883,{"$f":"F259*(1-Elteq!$F$8)","v":0.24517122521199883}]
["REIKU-B","PADSB-12",null,null,50,0.25807497390736728,{"$f":"F260*(1-Elteq!$F$8)","v":0.25807497390736728}]
["REIKU-B","PADSB-14/17",null,null,50,0.27097872260273559,{"$f":"F261*(1-Elteq!$F$8)","v":0.27097872260273559}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"PADSB-23",null,null,50,0.34840121477494562,{"$f":"F262*(1-Elteq!$F$8)","v":0.34840121477494562}]
["REIKU-B","PADSB-29",null,null,30,0.47743870172862929,{"$f":"F263*(1-Elteq!$F$8)","v":0.47743870172862929}]
["REIKU-B","PADSB-36",null,null,20,0.54195744520547118,{"$f":"F264*(1-Elteq!$F$8)","v":0.54195744520547118}]
["REIKU-B","PADSB-48",null,null,20,0.64518743476841811,{"$f":"F265*(1-Elteq!$F$8)","v":0.64518743476841811}]
["REIKU-B","PAEBB-70",null,null,10,4.7227720225048193,{"$f":"F266*(1-Elteq!$F$8)","v":4.7227720225048193}]
["REIKU-B","PAFHB-70",null,null,10,11.368202600619524,{"$f":"F267*(1-Elteq!$F$8)","v":11.368202600619524}]
["REIKU-B","PAFKB-52",null,null,10,14.726590905696076,{"$f":"F268*(1-Elteq!$F$8)","v":14.726590905696076}]
["REIKU-B","PAFKB-70",null,null,10,19.825329386338879,{"$f":"F269*(1-Elteq!$F$8)","v":19.825329386338879}]
["REIKU-B","PAFOB-07",null,null,50,1.0508895270304723,{"$f":"F270*(1-Elteq!$F$8)","v":1.0508895270304723}]
["REIKU-B","PAFOB-10",null,null,50,1.1702730906393146,{"$f":"F271*(1-Elteq!$F$8)","v":1.1702730906393146}]
["REIKU-B","PAFOB-12",null,null,50,1.3852813178624774,{"$f":"F272*(1-Elteq!$F$8)","v":1.3852813178624774}]
["REIKU-B","PAFOB-17",null,null,30,2.0516960425635697,{"$f":"F273*(1-Elteq!$F$8)","v":2.0516960425635697}]
["REIKU-B","PAFOB-23",null,null,30,3.3678784094911429,{"$f":"F274*(1-Elteq!$F$8)","v":3.3678784094911429}]
["REIKU-B","PAFOB-29",null,null,20,5.0453657398890277,{"$f":"F275*(1-Elteq!$F$8)","v":5.0453657398890277}]
["REIKU-B","PAFOB-36",null,null,10,7.4454629972275459,{"$f":"F276*(1-Elteq!$F$8)","v":7.4454629972275459}]
["REIKU-B","PAFOB-48",null,null,10,10.142346474559533,{"$f":"F277*(1-Elteq!$F$8)","v":10.142346474559533}]
["REIKU-B","PAFTB-70",null,null,10,11.368202600619524,{"$f":"F278*(1-Elteq!$F$8)","v":11.368202600619524}]
["REIKU-B","PAFVB-17",null,null,30,2.6581722312458824,{"$f":"F279*(1-Elteq!$F$8)","v":2.6581722312458824}]
["REIKU-B","PAFVB-23",null,null,30,4.2582370694715594,{"$f":"F280*(1-Elteq!$F$8)","v":4.2582370694715594}]
["REIKU-B","PAFVB-29",null,null,20,6.1937993737768124,{"$f":"F281*(1-Elteq!$F$8)","v":6.1937993737768124}]
["REIKU-B","PAFVB-36",null,null,10,9.122950327625432,{"$f":"F282*(1-Elteq!$F$8)","v":9.122950327625432}]
["REIKU-B","PAFVB-48",null,null,10,12.335983752772155,{"$f":"F283*(1-Elteq!$F$8)","v":12.335983752772155}]
["REIKU-B","PAGGB-70",null,null,10,43.811878825123323,{"$f":"F284*(1-Elteq!$F$8)","v":43.811878825123323}]
["REIKU-B","PAGGB-70i",null,null,10,13.796460869261766,{"$f":"F285*(1-Elteq!$F$8)","v":13.796460869261766}]
["REIKU-B","PAGGB-68i",null,null,10,13.796459424092316,{"$f":"F286*(1-Elteq!$F$8)","v":13.796459424092316}]
["REIKU-B","PAGHB-48",null,null,10,2.8646322103717763,{"$f":"F287*(1-Elteq!$F$8)","v":2.8646322103717763}]
["REIKU-B","PAGLB-36 ",null,null,10,3.3678784094911429,{"$f":"F288*(1-Elteq!$F$8)","v":3.3678784094911429}]
["REIKU-B","PAGLB-48 ",null,null,10,3.3678784094911429,{"$f":"F289*(1-Elteq!$F$8)","v":3.3678784094911429}]
["REIKU-B","PAGLB-52",null,null,10,3.3678784094911429,{"$f":"F290*(1-Elteq!$F$8)","v":3.3678784094911429}]
["REIKU-B","PAGLB-70",null,null,10,4.7227720225048193,{"$f":"F291*(1-Elteq!$F$8)","v":4.7227720225048193}]
["REIKU-B","PAGLB-70L",null,null,10,4.1550070799086116,{"$f":"F292*(1-Elteq!$F$8)","v":4.1550070799086116}]
["REIKU-B","PAGMG-07S22",null,null,50,1.9226585556098852,{"$f":"F293*(1-Elteq!$F$8)","v":1.9226585556098852}]
["REIKU-B","PAGMG-11S22",null,null,50,2.0904072886496752,{"$f":"F294*(1-Elteq!$F$8)","v":2.0904072886496752}]
["REIKU-B","PAGMG-20S32",null,null,50,2.7024832173318645,{"$f":"F295*(1-Elteq!$F$8)","v":2.7024832173318645}]
["REIKU-B","PAGMG-25S32",null,null,25,2.7024832173318645,{"$f":"F296*(1-Elteq!$F$8)","v":2.7024832173318645}]
["REIKU-B","PAGMG-32S40",null,null,25,3.3720173477519197,{"$f":"F297*(1-Elteq!$F$8)","v":3.3720173477519197}]
["REIKU-B","PAGMG-M12",null,null,100,0.19355623043052539,{"$f":"F298*(1-Elteq!$F$8)","v":0.19355623043052539}]
["REIKU-B","PAGMG-M16",null,null,100,0.20645997912589376,{"$f":"F299*(1-Elteq!$F$8)","v":0.20645997912589376}]
["REIKU-B","PAGMG-M20",null,null,100,0.30968996868884069,{"$f":"F300*(1-Elteq!$F$8)","v":0.30968996868884069}]
["REIKU-B","PAGMG-M25",null,null,100,0.32259371738420906,{"$f":"F301*(1-Elteq!$F$8)","v":0.32259371738420906}]
["REIKU-B","PAGMG-M32",null,null,50,0.70970617824526017,{"$f":"F302*(1-Elteq!$F$8)","v":0.70970617824526017}]
["REIKU-B","PAGMG-M40",null,null,25,1.0322998956294691,{"$f":"F303*(1-Elteq!$F$8)","v":1.0322998956294691}]
["REIKU-B","PAGMG-M50",null,null,25,1.3548936130136779,{"$f":"F304*(1-Elteq!$F$8)","v":1.3548936130136779}]
["REIKU-B","PAGMG-M63",null,null,25,1.5226423460534666,{"$f":"F305*(1-Elteq!$F$8)","v":1.5226423460534666}]
["REIKU-B","PAGMG-P07",null,null,100,0.14194123564905192,{"$f":"F306*(1-Elteq!$F$8)","v":0.14194123564905192}]
["REIKU-B","PAGMG-P09",null,null,100,0.15484498434442034,{"$f":"F307*(1-Elteq!$F$8)","v":0.15484498434442034}]
["REIKU-B","PAGMG-P11",null,null,100,0.16774873303978871,{"$f":"F308*(1-Elteq!$F$8)","v":0.16774873303978871}]
["REIKU-B","PAGMG-P13",null,null,100,0.18065248173515702,{"$f":"F309*(1-Elteq!$F$8)","v":0.18065248173515702}]
["REIKU-B","PAGMG-P16",null,null,100,0.19355623043052539,{"$f":"F310*(1-Elteq!$F$8)","v":0.19355623043052539}]
["REIKU-B","PAGMG-P21",null,null,100,0.30968996868884069,{"$f":"F311*(1-Elteq!$F$8)","v":0.30968996868884069}]
["REIKU-B","PAGMG-P29",null,null,100,0.69680242954989124,{"$f":"F312*(1-Elteq!$F$8)","v":0.69680242954989124}]
["REIKU-B","PAGMG-P36",null,null,25,1.3161823669275732,{"$f":"F313*(1-Elteq!$F$8)","v":1.3161823669275732}]
["REIKU-B","PAGMG-P42",null,null,25,1.3936048590997825,{"$f":"F314*(1-Elteq!$F$8)","v":1.3936048590997825}]
["REIKU-B","PAGMG-P48",null,null,25,1.3936048590997825,{"$f":"F315*(1-Elteq!$F$8)","v":1.3936048590997825}]
["REIKU-B","PAGOB-07G00",null,null,50,1.0072988179496118,{"$f":"F316*(1-Elteq!$F$8)","v":1.0072988179496118}]
["REIKU-B","PAGOB-07M101",null,null,50,1.0072988179496118,{"$f":"F317*(1-Elteq!$F$8)","v":1.0072988179496118}]
["REIKU-B","PAGOB-07M12",null,null,50,1.0072988179496118,{"$f":"F318*(1-Elteq!$F$8)","v":1.0072988179496118}]
["REIKU-B","PAGOB-07M12Z",null,null,30,2.6065572364644094,{"$f":"F319*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-B","PAGOB-07M16",null,null,50,1.0072988179496118,{"$f":"F320*(1-Elteq!$F$8)","v":1.0072988179496118}]
["REIKU-B","PAGOB-07M20",null,null,50,1.0072988179496118,{"$f":"F321*(1-Elteq!$F$8)","v":1.0072988179496118}]
["REIKU-B","PAGOB-07P07",null,null,50,1.0072988179496118,{"$f":"F322*(1-Elteq!$F$8)","v":1.0072988179496118}]
["REIKU-B","PAGOB-07P07Z",null,null,30,2.6065572364644094,{"$f":"F323*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-B","PAGOB-07P09",null,null,50,1.0072988179496118,{"$f":"F324*(1-Elteq!$F$8)","v":1.0072988179496118}]
["REIKU-B","PAGOB-07P11",null,null,50,1.0072988179496118,{"$f":"F325*(1-Elteq!$F$8)","v":1.0072988179496118}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"PAGOB-07P13",null,null,50,1.0072988179496118,{"$f":"F326*(1-Elteq!$F$8)","v":1.0072988179496118}]
["REIKU-B","PAGOB-07S13",null,null,50,1.1604553633688508,{"$f":"F327*(1-Elteq!$F$8)","v":1.1604553633688508}]
["REIKU-B","PAGOB-10M12",null,null,50,1.1015489997460666,{"$f":"F328*(1-Elteq!$F$8)","v":1.1015489997460666}]
["REIKU-B","PAGOB-10M16",null,null,50,1.1015489997460666,{"$f":"F329*(1-Elteq!$F$8)","v":1.1015489997460666}]
["REIKU-B","PAGOB-10M16Z",null,null,30,3.1356109329745108,{"$f":"F330*(1-Elteq!$F$8)","v":3.1356109329745108}]
["REIKU-B","PAGOB-10M20",null,null,50,1.1015489997460666,{"$f":"F331*(1-Elteq!$F$8)","v":1.1015489997460666}]
["REIKU-B","PAGOB-10P07",null,null,50,1.0308613633987256,{"$f":"F332*(1-Elteq!$F$8)","v":1.0308613633987256}]
["REIKU-B","PAGOB-10P09",null,null,50,1.0308613633987256,{"$f":"F333*(1-Elteq!$F$8)","v":1.0308613633987256}]
["REIKU-B","PAGOB-10P09Z",null,null,30,2.8775359590671443,{"$f":"F334*(1-Elteq!$F$8)","v":2.8775359590671443}]
["REIKU-B","PAGOB-10P11",null,null,50,1.1015489997460666,{"$f":"F335*(1-Elteq!$F$8)","v":1.1015489997460666}]
["REIKU-B","PAGOB-10P13",null,null,50,1.1015489997460666,{"$f":"F336*(1-Elteq!$F$8)","v":1.1015489997460666}]
["REIKU-B","PAGOB-10S15",null,null,50,1.1722366360934076,{"$f":"F337*(1-Elteq!$F$8)","v":1.1722366360934076}]
["REIKU-B","PAGOB-12M16",null,null,50,1.1015489997460666,{"$f":"F338*(1-Elteq!$F$8)","v":1.1015489997460666}]
["REIKU-B","PAGOB-12M16Z",null,null,30,3.2904559173189316,{"$f":"F339*(1-Elteq!$F$8)","v":3.2904559173189316}]
["REIKU-B","PAGOB-12M20",null,null,50,1.1015489997460666,{"$f":"F340*(1-Elteq!$F$8)","v":1.1015489997460666}]
["REIKU-B","PAGOB-12M20Z",null,null,30,3.2904559173189316,{"$f":"F341*(1-Elteq!$F$8)","v":3.2904559173189316}]
["REIKU-B","PAGOB-12P09",null,null,50,1.1015489997460666,{"$f":"F342*(1-Elteq!$F$8)","v":1.1015489997460666}]
["REIKU-B","PAGOB-12P11",null,null,50,1.1015489997460666,{"$f":"F343*(1-Elteq!$F$8)","v":1.1015489997460666}]
["REIKU-B","PAGOB-12P11Z",null,null,30,2.9936696973254597,{"$f":"F344*(1-Elteq!$F$8)","v":2.9936696973254597}]
["REIKU-B","PAGOB-12P13",null,null,50,1.1015489997460666,{"$f":"F345*(1-Elteq!$F$8)","v":1.1015489997460666}]
["REIKU-B","PAGOB-12P13Z",null,null,30,3.0194771947161958,{"$f":"F346*(1-Elteq!$F$8)","v":3.0194771947161958}]
["REIKU-B","PAGOB-12S19",null,null,50,1.1840179088179645,{"$f":"F347*(1-Elteq!$F$8)","v":1.1840179088179645}]
["REIKU-B","PAGOB-17M20",null,null,50,1.1133302724706238,{"$f":"F348*(1-Elteq!$F$8)","v":1.1133302724706238}]
["REIKU-B","PAGOB-17M20Z",null,null,30,3.9098358546966128,{"$f":"F349*(1-Elteq!$F$8)","v":3.9098358546966128}]
["REIKU-B","PAGOB-17M25",null,null,50,1.1133302724706238,{"$f":"F350*(1-Elteq!$F$8)","v":1.1133302724706238}]
["REIKU-B","PAGOB-17M32",null,null,50,1.1133302724706238,{"$f":"F351*(1-Elteq!$F$8)","v":1.1133302724706238}]
["REIKU-B","PAGOB-17P11",null,null,50,1.1133302724706238,{"$f":"F352*(1-Elteq!$F$8)","v":1.1133302724706238}]
["REIKU-B","PAGOB-17P13",null,null,50,1.1133302724706238,{"$f":"F353*(1-Elteq!$F$8)","v":1.1133302724706238}]
["REIKU-B","PAGOB-17P16",null,null,50,1.1133302724706238,{"$f":"F354*(1-Elteq!$F$8)","v":1.1133302724706238}]
["REIKU-B","PAGOB-17P16Z",null,null,30,3.5614346399216661,{"$f":"F355*(1-Elteq!$F$8)","v":3.5614346399216661}]
["REIKU-B","PAGOB-17P21",null,null,50,1.7534460905048797,{"$f":"F356*(1-Elteq!$F$8)","v":1.7534460905048797}]
["REIKU-B","PAGOB-17S22",null,null,50,1.1957991815425215,{"$f":"F357*(1-Elteq!$F$8)","v":1.1957991815425215}]
["REIKU-B","PAGOB-23M25",null,null,30,1.7770086359539934,{"$f":"F358*(1-Elteq!$F$8)","v":1.7770086359539934}]
["REIKU-B","PAGOB-23M25Z",null,null,30,4.7614832685909265,{"$f":"F359*(1-Elteq!$F$8)","v":4.7614832685909265}]
["REIKU-B","PAGOB-23M32",null,null,30,1.7770086359539934,{"$f":"F360*(1-Elteq!$F$8)","v":1.7770086359539934}]
["REIKU-B","PAGOB-23P16",null,null,50,1.7887899086785501,{"$f":"F361*(1-Elteq!$F$8)","v":1.7887899086785501}]
["REIKU-B","PAGOB-23P21",null,null,30,1.7887899086785501,{"$f":"F362*(1-Elteq!$F$8)","v":1.7887899086785501}]
["REIKU-B","PAGOB-23P21Z",null,null,30,4.3743708077298731,{"$f":"F363*(1-Elteq!$F$8)","v":4.3743708077298731}]
["REIKU-B","PAGOB-23S28",null,null,30,2.1088478176956786,{"$f":"F364*(1-Elteq!$F$8)","v":2.1088478176956786}]
["REIKU-B","PAGOB-23S32",null,null,30,2.1088478176956786,{"$f":"F365*(1-Elteq!$F$8)","v":2.1088478176956786}]
["REIKU-B","PAGOB-29M32",null,null,30,2.3444732721868151,{"$f":"F366*(1-Elteq!$F$8)","v":2.3444732721868151}]
["REIKU-B","PAGOB-29M32Z",null,null,20,6.2841256146443927,{"$f":"F367*(1-Elteq!$F$8)","v":6.2841256146443927}]
["REIKU-B","PAGOB-29M40",null,null,30,2.3444732721868151,{"$f":"F368*(1-Elteq!$F$8)","v":2.3444732721868151}]
["REIKU-B","PAGOB-29P29",null,null,30,2.3444732721868151,{"$f":"F369*(1-Elteq!$F$8)","v":2.3444732721868151}]
["REIKU-B","PAGOB-29P29Z",null,null,20,5.8453981590018671,{"$f":"F370*(1-Elteq!$F$8)","v":5.8453981590018671}]
["REIKU-B","PAGOB-29S37",null,null,30,3.0808028174716195,{"$f":"F371*(1-Elteq!$F$8)","v":3.0808028174716195}]
["REIKU-B","PAGOB-29S40",null,null,30,3.0808028174716195,{"$f":"F372*(1-Elteq!$F$8)","v":3.0808028174716195}]
["REIKU-B","PAGOB-36M40",null,null,10,4.0036691808952414,{"$f":"F373*(1-Elteq!$F$8)","v":4.0036691808952414}]
["REIKU-B","PAGOB-36M40Z",null,null,10,11.832737553652786,{"$f":"F374*(1-Elteq!$F$8)","v":11.832737553652786}]
["REIKU-B","PAGOB-36M50",null,null,10,4.0036691808952414,{"$f":"F375*(1-Elteq!$F$8)","v":4.0036691808952414}]
["REIKU-B","PAGOB-36P29",null,null,10,4.0036691808952414,{"$f":"F376*(1-Elteq!$F$8)","v":4.0036691808952414}]
["REIKU-B","PAGOB-36P36",null,null,10,4.0036691808952414,{"$f":"F377*(1-Elteq!$F$8)","v":4.0036691808952414}]
["REIKU-B","PAGOB-36P36Z",null,null,10,11.832737553652786,{"$f":"F378*(1-Elteq!$F$8)","v":11.832737553652786}]
["REIKU-B","PAGOB-48M50",null,null,10,5.2112496351623179,{"$f":"F379*(1-Elteq!$F$8)","v":5.2112496351623179}]
["REIKU-B","PAGOB-48M63",null,null,10,5.2112496351623179,{"$f":"F380*(1-Elteq!$F$8)","v":5.2112496351623179}]
["REIKU-B","PAGOB-48M63Z",null,null,10,13.587647376222883,{"$f":"F381*(1-Elteq!$F$8)","v":13.587647376222883}]
["REIKU-B","PAGOB-48P42",null,null,10,5.2112496351623179,{"$f":"F382*(1-Elteq!$F$8)","v":5.2112496351623179}]
["REIKU-B","PAGOB-48P48",null,null,10,5.2112496351623179,{"$f":"F383*(1-Elteq!$F$8)","v":5.2112496351623179}]
["REIKU-B","PAGOB-48P48Z",null,null,10,13.587647376222883,{"$f":"F384*(1-Elteq!$F$8)","v":13.587647376222883}]
["REIKU-B","PAGOB-42",null,null,10,7.2258472710615402,{"$f":"F385*(1-Elteq!$F$8)","v":7.2258472710615402}]
["REIKU-B","PAGOB-52",null,null,10,9.4642890887273463,{"$f":"F386*(1-Elteq!$F$8)","v":9.4642890887273463}]
["REIKU-B","PAGOB-70",null,null,10,10.471587906676957,{"$f":"F387*(1-Elteq!$F$8)","v":10.471587906676957}]
["REIKU-B","PAGOB-95",null,null,10,12.757154815240989,{"$f":"F388*(1-Elteq!$F$8)","v":12.757154815240989}]
["REIKU-B","PAGPB-52",null,null,10,7.7304784527633936,{"$f":"F389*(1-Elteq!$F$8)","v":7.7304784527633936}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"PAGVB-07M101",null,null,50,1.4323161051858881,{"$f":"F390*(1-Elteq!$F$8)","v":1.4323161051858881}]
["REIKU-B","PAGVB-07M12",null,null,50,1.4452198538812562,{"$f":"F391*(1-Elteq!$F$8)","v":1.4452198538812562}]
["REIKU-B","PAGVB-07M12Z",null,null,30,2.9549584512393556,{"$f":"F392*(1-Elteq!$F$8)","v":2.9549584512393556}]
["REIKU-B","PAGVB-07M16",null,null,50,1.4581236025766247,{"$f":"F393*(1-Elteq!$F$8)","v":1.4581236025766247}]
["REIKU-B","PAGVB-07M20",null,null,50,1.4968348486627299,{"$f":"F394*(1-Elteq!$F$8)","v":1.4968348486627299}]
["REIKU-B","PAGVB-07P07",null,null,50,1.4452198538812562,{"$f":"F395*(1-Elteq!$F$8)","v":1.4452198538812562}]
["REIKU-B","PAGVB-07P07Z",null,null,30,2.9549584512393556,{"$f":"F396*(1-Elteq!$F$8)","v":2.9549584512393556}]
["REIKU-B","PAGVB-07P09",null,null,50,1.4452198538812562,{"$f":"F397*(1-Elteq!$F$8)","v":1.4452198538812562}]
["REIKU-B","PAGVB-07P11",null,null,50,1.4581236025766247,{"$f":"F398*(1-Elteq!$F$8)","v":1.4581236025766247}]
["REIKU-B","PAGVB-07P13",null,null,50,1.4839310999673616,{"$f":"F399*(1-Elteq!$F$8)","v":1.4839310999673616}]
["REIKU-B","PAGVB-10M12",null,null,50,1.5613535921395714,{"$f":"F400*(1-Elteq!$F$8)","v":1.5613535921395714}]
["REIKU-B","PAGVB-10M16",null,null,50,1.5742573408349396,{"$f":"F401*(1-Elteq!$F$8)","v":1.5742573408349396}]
["REIKU-B","PAGVB-10M16Z",null,null,30,3.5098196451401935,{"$f":"F402*(1-Elteq!$F$8)","v":3.5098196451401935}]
["REIKU-B","PAGVB-10M20",null,null,50,1.6129685869210446,{"$f":"F403*(1-Elteq!$F$8)","v":1.6129685869210446}]
["REIKU-B","PAGVB-10P07",null,null,50,1.4839310999673616,{"$f":"F404*(1-Elteq!$F$8)","v":1.4839310999673616}]
["REIKU-B","PAGVB-10P09",null,null,50,1.4839310999673616,{"$f":"F405*(1-Elteq!$F$8)","v":1.4839310999673616}]
["REIKU-B","PAGVB-10P09Z",null,null,30,3.238840922537459,{"$f":"F406*(1-Elteq!$F$8)","v":3.238840922537459}]
["REIKU-B","PAGVB-10P11",null,null,50,1.5742573408349396,{"$f":"F407*(1-Elteq!$F$8)","v":1.5742573408349396}]
["REIKU-B","PAGVB-10P13",null,null,50,1.5871610895303083,{"$f":"F408*(1-Elteq!$F$8)","v":1.5871610895303083}]
["REIKU-B","PAGVB-12M16",null,null,50,1.5871610895303083,{"$f":"F409*(1-Elteq!$F$8)","v":1.5871610895303083}]
["REIKU-B","PAGVB-12M16Z",null,null,30,3.6775683781799819,{"$f":"F410*(1-Elteq!$F$8)","v":3.6775683781799819}]
["REIKU-B","PAGVB-12M20",null,null,50,1.6258723356164138,{"$f":"F411*(1-Elteq!$F$8)","v":1.6258723356164138}]
["REIKU-B","PAGVB-12M20Z",null,null,30,3.7162796242660856,{"$f":"F412*(1-Elteq!$F$8)","v":3.7162796242660856}]
["REIKU-B","PAGVB-12P09",null,null,50,1.5742573408349396,{"$f":"F413*(1-Elteq!$F$8)","v":1.5742573408349396}]
["REIKU-B","PAGVB-12P11",null,null,50,1.5871610895303083,{"$f":"F414*(1-Elteq!$F$8)","v":1.5871610895303083}]
["REIKU-B","PAGVB-12P11Z",null,null,30,3.3678784094911429,{"$f":"F415*(1-Elteq!$F$8)","v":3.3678784094911429}]
["REIKU-B","PAGVB-12P13",null,null,50,1.6000648382256766,{"$f":"F416*(1-Elteq!$F$8)","v":1.6000648382256766}]
["REIKU-B","PAGVB-12P13Z",null,null,30,3.4065896555772461,{"$f":"F417*(1-Elteq!$F$8)","v":3.4065896555772461}]
["REIKU-B","PAGVB-17M20",null,null,50,1.65167983300715,{"$f":"F418*(1-Elteq!$F$8)","v":1.65167983300715}]
["REIKU-B","PAGVB-17M20Z",null,null,30,4.3485633103391379,{"$f":"F419*(1-Elteq!$F$8)","v":4.3485633103391379}]
["REIKU-B","PAGVB-17M25",null,null,50,1.6774873303978866,{"$f":"F420*(1-Elteq!$F$8)","v":1.6774873303978866}]
["REIKU-B","PAGVB-17M32",null,null,50,1.7678135712654652,{"$f":"F421*(1-Elteq!$F$8)","v":1.7678135712654652}]
["REIKU-B","PAGVB-17P11",null,null,50,1.6774873303978866,{"$f":"F422*(1-Elteq!$F$8)","v":1.6774873303978866}]
["REIKU-B","PAGVB-17P13",null,null,50,1.6258723356164138,{"$f":"F423*(1-Elteq!$F$8)","v":1.6258723356164138}]
["REIKU-B","PAGVB-17P16",null,null,50,1.638776084311782,{"$f":"F424*(1-Elteq!$F$8)","v":1.638776084311782}]
["REIKU-B","PAGVB-17P16Z",null,null,30,3.9872583468688241,{"$f":"F425*(1-Elteq!$F$8)","v":3.9872583468688241}]
["REIKU-B","PAGVB-17P21",null,null,50,2.3613860112524097,{"$f":"F426*(1-Elteq!$F$8)","v":2.3613860112524097}]
["REIKU-B","PAGVB-23M25",null,null,30,2.5807497390736724,{"$f":"F427*(1-Elteq!$F$8)","v":2.5807497390736724}]
["REIKU-B","PAGVB-23M25Z",null,null,30,5.4066707033593433,{"$f":"F428*(1-Elteq!$F$8)","v":5.4066707033593433}]
["REIKU-B","PAGVB-23M32",null,null,30,2.6710759799412513,{"$f":"F429*(1-Elteq!$F$8)","v":2.6710759799412513}]
["REIKU-B","PAGVB-23P16",null,null,50,2.5549422416829355,{"$f":"F430*(1-Elteq!$F$8)","v":2.5549422416829355}]
["REIKU-B","PAGVB-23P21",null,null,30,2.5936534877690405,{"$f":"F431*(1-Elteq!$F$8)","v":2.5936534877690405}]
["REIKU-B","PAGVB-23P21Z",null,null,30,5.0324619911936601,{"$f":"F432*(1-Elteq!$F$8)","v":5.0324619911936601}]
["REIKU-B","PAGVB-29M32",null,null,30,3.3936859068818794,{"$f":"F433*(1-Elteq!$F$8)","v":3.3936859068818794}]
["REIKU-B","PAGVB-29M32Z",null,null,20,7.1228692798433322,{"$f":"F434*(1-Elteq!$F$8)","v":7.1228692798433322}]
["REIKU-B","PAGVB-29M40",null,null,30,3.5743383886170359,{"$f":"F435*(1-Elteq!$F$8)","v":3.5743383886170359}]
["REIKU-B","PAGVB-29P29",null,null,30,3.3936859068818794,{"$f":"F436*(1-Elteq!$F$8)","v":3.3936859068818794}]
["REIKU-B","PAGVB-29P29Z",null,null,20,6.6970455728961822,{"$f":"F437*(1-Elteq!$F$8)","v":6.6970455728961822}]
["REIKU-B","PAGVB-36M40",null,null,10,5.6647456772667102,{"$f":"F438*(1-Elteq!$F$8)","v":5.6647456772667102}]
["REIKU-B","PAGVB-36M40Z",null,null,10,13.136016171884989,{"$f":"F439*(1-Elteq!$F$8)","v":13.136016171884989}]
["REIKU-B","PAGVB-36M50",null,null,10,5.8712056563926049,{"$f":"F440*(1-Elteq!$F$8)","v":5.8712056563926049}]
["REIKU-B","PAGVB-36P29",null,null,10,5.4840931955315542,{"$f":"F441*(1-Elteq!$F$8)","v":5.4840931955315542}]
["REIKU-B","PAGVB-36P36",null,null,10,5.5615156877037641,{"$f":"F442*(1-Elteq!$F$8)","v":5.5615156877037641}]
["REIKU-B","PAGVB-36P36Z",null,null,10,13.032786182322042,{"$f":"F443*(1-Elteq!$F$8)","v":13.032786182322042}]
["REIKU-B","PAGVB-48M50",null,null,10,7.3680405050553359,{"$f":"F444*(1-Elteq!$F$8)","v":7.3680405050553359}]
["REIKU-B","PAGVB-48M63",null,null,10,7.5615967354858586,{"$f":"F445*(1-Elteq!$F$8)","v":7.5615967354858586}]
["REIKU-B","PAGVB-48M63Z",null,null,10,15.497402183137401,{"$f":"F446*(1-Elteq!$F$8)","v":15.497402183137401}]
["REIKU-B","PAGVB-48P42",null,null,10,7.6519229763534371,{"$f":"F447*(1-Elteq!$F$8)","v":7.6519229763534371}]
["REIKU-B","PAGVB-48P48",null,null,10,7.1228692798433322,{"$f":"F448*(1-Elteq!$F$8)","v":7.1228692798433322}]
["REIKU-B","PAGVB-48P48Z",null,null,10,15.032867230104134,{"$f":"F449*(1-Elteq!$F$8)","v":15.032867230104134}]
["REIKU-B","PAHDB-07",null,null,100,0.65809118346378659,{"$f":"F450*(1-Elteq!$F$8)","v":0.65809118346378659}]
["REIKU-B","PAHDB-10",null,null,100,0.67099493215915484,{"$f":"F451*(1-Elteq!$F$8)","v":0.67099493215915484}]
["REIKU-B","PAHDB-12",null,null,50,0.69680242954989124,{"$f":"F452*(1-Elteq!$F$8)","v":0.69680242954989124}]
["REIKU-B","PAHDB-14",null,null,50,0.74841742433136493,{"$f":"F453*(1-Elteq!$F$8)","v":0.74841742433136493}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"PAHDB-17",null,null,50,0.7613211730267333,{"$f":"F454*(1-Elteq!$F$8)","v":0.7613211730267333}]
["REIKU-B","PAHDB-23",null,null,50,1.3807011104044142,{"$f":"F455*(1-Elteq!$F$8)","v":1.3807011104044142}]
["REIKU-B","PAHDB-29",null,null,30,1.7420060738747289,{"$f":"F456*(1-Elteq!$F$8)","v":1.7420060738747289}]
["REIKU-B","PAHDB-36",null,null,20,2.2194447756033582,{"$f":"F457*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-B","PAHDB-48",null,null,20,2.8646322103717763,{"$f":"F458*(1-Elteq!$F$8)","v":2.8646322103717763}]
["REIKU-B","PAHOB-07",null,null,100,0.41291995825178751,{"$f":"F459*(1-Elteq!$F$8)","v":0.41291995825178751}]
["REIKU-B","PAHOB-10",null,null,100,0.42582370694715577,{"$f":"F460*(1-Elteq!$F$8)","v":0.42582370694715577}]
["REIKU-B","PAHOB-12",null,null,50,0.43872745564252419,{"$f":"F461*(1-Elteq!$F$8)","v":0.43872745564252419}]
["REIKU-B","PAHOB-14",null,null,50,0.47743870172862929,{"$f":"F462*(1-Elteq!$F$8)","v":0.47743870172862929}]
["REIKU-B","PAHOB-17",null,null,50,0.49034245042399766,{"$f":"F463*(1-Elteq!$F$8)","v":0.49034245042399766}]
["REIKU-B","PAHOB-17S",null,null,50,0.49034245042399766,{"$f":"F464*(1-Elteq!$F$8)","v":0.49034245042399766}]
["REIKU-B","PAHOB-23",null,null,50,1.0322998956294691,{"$f":"F465*(1-Elteq!$F$8)","v":1.0322998956294691}]
["REIKU-B","PAHOB-23S",null,null,50,1.0322998956294691,{"$f":"F466*(1-Elteq!$F$8)","v":1.0322998956294691}]
["REIKU-B","PAHOB-29",null,null,30,1.264567372146099,{"$f":"F467*(1-Elteq!$F$8)","v":1.264567372146099}]
["REIKU-B","PAHOB-29S",null,null,30,1.264567372146099,{"$f":"F468*(1-Elteq!$F$8)","v":1.264567372146099}]
["REIKU-B","PAHOB-36",null,null,20,1.6774873303978866,{"$f":"F469*(1-Elteq!$F$8)","v":1.6774873303978866}]
["REIKU-B","PAHOB-36S",null,null,20,1.6774873303978866,{"$f":"F470*(1-Elteq!$F$8)","v":1.6774873303978866}]
["REIKU-B","PAHOB-36V",null,null,20,1.6774873303978866,{"$f":"F471*(1-Elteq!$F$8)","v":1.6774873303978866}]
["REIKU-B","PAHOB-48",null,null,20,2.2194447756033582,{"$f":"F472*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-B","PAHOB-48S",null,null,20,2.2194447756033582,{"$f":"F473*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-B","PAHOB-48V",null,null,20,2.2194447756033582,{"$f":"F474*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-B","PAIOB-07M081",null,null,50,1.72910232517936,{"$f":"F475*(1-Elteq!$F$8)","v":1.72910232517936}]
["REIKU-B","PAIOB-07M121",null,null,50,1.72910232517936,{"$f":"F476*(1-Elteq!$F$8)","v":1.72910232517936}]
["REIKU-B","PAIOB-07M16",null,null,50,1.72910232517936,{"$f":"F477*(1-Elteq!$F$8)","v":1.72910232517936}]
["REIKU-B","PAIOB-07P07",null,null,50,1.72910232517936,{"$f":"F478*(1-Elteq!$F$8)","v":1.72910232517936}]
["REIKU-B","PAIOB-07U05",null,null,50,1.9484660530006226,{"$f":"F479*(1-Elteq!$F$8)","v":1.9484660530006226}]
["REIKU-B","PAIOB-10M121",null,null,50,1.72910232517936,{"$f":"F480*(1-Elteq!$F$8)","v":1.72910232517936}]
["REIKU-B","PAIOB-10M16",null,null,50,1.72910232517936,{"$f":"F481*(1-Elteq!$F$8)","v":1.72910232517936}]
["REIKU-B","PAIOB-10M181",null,null,50,1.72910232517936,{"$f":"F482*(1-Elteq!$F$8)","v":1.72910232517936}]
["REIKU-B","PAIOB-10P07",null,null,50,1.72910232517936,{"$f":"F483*(1-Elteq!$F$8)","v":1.72910232517936}]
["REIKU-B","PAIOB-10P09",null,null,50,1.72910232517936,{"$f":"F484*(1-Elteq!$F$8)","v":1.72910232517936}]
["REIKU-B","PAIOB-10U05",null,null,50,1.9484660530006226,{"$f":"F485*(1-Elteq!$F$8)","v":1.9484660530006226}]
["REIKU-B","PAIOB-10U07",null,null,50,1.9484660530006226,{"$f":"F486*(1-Elteq!$F$8)","v":1.9484660530006226}]
["REIKU-B","PAIOB-12M16",null,null,50,1.7678135712654652,{"$f":"F487*(1-Elteq!$F$8)","v":1.7678135712654652}]
["REIKU-B","PAIOB-12M20",null,null,50,1.7678135712654652,{"$f":"F488*(1-Elteq!$F$8)","v":1.7678135712654652}]
["REIKU-B","PAIOB-12P11",null,null,50,1.7678135712654652,{"$f":"F489*(1-Elteq!$F$8)","v":1.7678135712654652}]
["REIKU-B","PAIOB-12P13",null,null,50,1.7678135712654652,{"$f":"F490*(1-Elteq!$F$8)","v":1.7678135712654652}]
["REIKU-B","PAIOB-12U05",null,null,50,2.0129847964774643,{"$f":"F491*(1-Elteq!$F$8)","v":2.0129847964774643}]
["REIKU-B","PAIOB-12U06",null,null,50,2.0129847964774643,{"$f":"F492*(1-Elteq!$F$8)","v":2.0129847964774643}]
["REIKU-B","PAIOB-12U07",null,null,50,2.0129847964774643,{"$f":"F493*(1-Elteq!$F$8)","v":2.0129847964774643}]
["REIKU-B","PAIOB-12U09",null,null,50,2.0129847964774643,{"$f":"F494*(1-Elteq!$F$8)","v":2.0129847964774643}]
["REIKU-B","PAIOB-12U10",null,null,50,2.0129847964774643,{"$f":"F495*(1-Elteq!$F$8)","v":2.0129847964774643}]
["REIKU-B","PAIOB-17M20",null,null,50,1.8323323147423072,{"$f":"F496*(1-Elteq!$F$8)","v":1.8323323147423072}]
["REIKU-B","PAIOB-17P13",null,null,50,1.8323323147423072,{"$f":"F497*(1-Elteq!$F$8)","v":1.8323323147423072}]
["REIKU-B","PAIOB-17P16",null,null,50,1.8323323147423072,{"$f":"F498*(1-Elteq!$F$8)","v":1.8323323147423072}]
["REIKU-B","PAIOB-17U07",null,null,50,2.0645997912589382,{"$f":"F499*(1-Elteq!$F$8)","v":2.0645997912589382}]
["REIKU-B","PAIOB-17U09",null,null,50,2.0645997912589382,{"$f":"F500*(1-Elteq!$F$8)","v":2.0645997912589382}]
["REIKU-B","PAIOB-17U10",null,null,50,2.0645997912589382,{"$f":"F501*(1-Elteq!$F$8)","v":2.0645997912589382}]
["REIKU-B","PAIOB-17U11",null,null,50,2.0645997912589382,{"$f":"F502*(1-Elteq!$F$8)","v":2.0645997912589382}]
["REIKU-B","PAIOB-17U14",null,null,50,2.0645997912589382,{"$f":"F503*(1-Elteq!$F$8)","v":2.0645997912589382}]
["REIKU-B","PAIOB-17U17",null,null,50,2.0645997912589382,{"$f":"F504*(1-Elteq!$F$8)","v":2.0645997912589382}]
["REIKU-B","PAIOB-23M25",null,null,30,3.8711246086105069,{"$f":"F505*(1-Elteq!$F$8)","v":3.8711246086105069}]
["REIKU-B","PAIOB-23P21",null,null,30,3.8711246086105069,{"$f":"F506*(1-Elteq!$F$8)","v":3.8711246086105069}]
["REIKU-B","PAIOB-23U14",null,null,30,4.3614670590345064,{"$f":"F507*(1-Elteq!$F$8)","v":4.3614670590345064}]
["REIKU-B","PAIOB-23U17",null,null,30,4.3614670590345064,{"$f":"F508*(1-Elteq!$F$8)","v":4.3614670590345064}]
["REIKU-B","PAIOB-23U18",null,null,30,4.3614670590345064,{"$f":"F509*(1-Elteq!$F$8)","v":4.3614670590345064}]
["REIKU-B","PAIOB-29M32",null,null,30,6.555104337247128,{"$f":"F510*(1-Elteq!$F$8)","v":6.555104337247128}]
["REIKU-B","PAIOB-29P29",null,null,30,6.3815227258016343,{"$f":"F511*(1-Elteq!$F$8)","v":6.3815227258016343}]
["REIKU-B","PAIOB-29U24",null,null,30,6.5422005885517578,{"$f":"F512*(1-Elteq!$F$8)","v":6.5422005885517578}]
["REIKU-B","PAIOB-36M40",null,null,10,6.6196230807239651,{"$f":"F513*(1-Elteq!$F$8)","v":6.6196230807239651}]
["REIKU-B","PAIOB-36P36",null,null,10,6.6196230807239651,{"$f":"F514*(1-Elteq!$F$8)","v":6.6196230807239651}]
["REIKU-B","PAIOB-48M50",null,null,10,12.400502496248995,{"$f":"F515*(1-Elteq!$F$8)","v":12.400502496248995}]
["REIKU-B","PAIOB-48P48",null,null,10,12.400502496248995,{"$f":"F516*(1-Elteq!$F$8)","v":12.400502496248995}]
["REIKU-B","PAIRB-07M081",null,null,50,1.9226585556098852,{"$f":"F517*(1-Elteq!$F$8)","v":1.9226585556098852}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"PAIRB-07M121",null,null,50,1.9226585556098852,{"$f":"F518*(1-Elteq!$F$8)","v":1.9226585556098852}]
["REIKU-B","PAIRB-07M16",null,null,50,1.9226585556098852,{"$f":"F519*(1-Elteq!$F$8)","v":1.9226585556098852}]
["REIKU-B","PAIRB-07P07",null,null,50,1.9226585556098852,{"$f":"F520*(1-Elteq!$F$8)","v":1.9226585556098852}]
["REIKU-B","PAIRB-10M121",null,null,50,1.9355623043052534,{"$f":"F521*(1-Elteq!$F$8)","v":1.9355623043052534}]
["REIKU-B","PAIRB-10M16",null,null,50,1.9355623043052534,{"$f":"F522*(1-Elteq!$F$8)","v":1.9355623043052534}]
["REIKU-B","PAIRB-10M181",null,null,50,1.9355623043052534,{"$f":"F523*(1-Elteq!$F$8)","v":1.9355623043052534}]
["REIKU-B","PAIRB-10P07",null,null,50,1.9355623043052534,{"$f":"F524*(1-Elteq!$F$8)","v":1.9355623043052534}]
["REIKU-B","PAIRB-10P09",null,null,50,1.9355623043052534,{"$f":"F525*(1-Elteq!$F$8)","v":1.9355623043052534}]
["REIKU-B","PAIRB-12M16",null,null,50,1.987177299086728,{"$f":"F526*(1-Elteq!$F$8)","v":1.987177299086728}]
["REIKU-B","PAIRB-12M20",null,null,50,1.987177299086728,{"$f":"F527*(1-Elteq!$F$8)","v":1.987177299086728}]
["REIKU-B","PAIRB-12P11",null,null,50,1.987177299086728,{"$f":"F528*(1-Elteq!$F$8)","v":1.987177299086728}]
["REIKU-B","PAIRB-12P13",null,null,50,1.987177299086728,{"$f":"F529*(1-Elteq!$F$8)","v":1.987177299086728}]
["REIKU-B","PAIRB-17M20",null,null,50,2.0645997912589382,{"$f":"F530*(1-Elteq!$F$8)","v":2.0645997912589382}]
["REIKU-B","PAIRB-17P13",null,null,50,2.0645997912589382,{"$f":"F531*(1-Elteq!$F$8)","v":2.0645997912589382}]
["REIKU-B","PAIRB-17P16",null,null,50,2.0645997912589382,{"$f":"F532*(1-Elteq!$F$8)","v":2.0645997912589382}]
["REIKU-B","PAIRB-23M25",null,null,30,4.2840445668622964,{"$f":"F533*(1-Elteq!$F$8)","v":4.2840445668622964}]
["REIKU-B","PAIRB-23P21",null,null,30,4.2840445668622964,{"$f":"F534*(1-Elteq!$F$8)","v":4.2840445668622964}]
["REIKU-B","PAIRB-29M32",null,null,30,7.0712542850618609,{"$f":"F535*(1-Elteq!$F$8)","v":7.0712542850618609}]
["REIKU-B","PAIRB-29P29",null,null,30,7.0712542850618609,{"$f":"F536*(1-Elteq!$F$8)","v":7.0712542850618609}]
["REIKU-B","PAIRB-36M40",null,null,10,7.4067517511414405,{"$f":"F537*(1-Elteq!$F$8)","v":7.4067517511414405}]
["REIKU-B","PAIRB-36P36",null,null,10,7.4067517511414405,{"$f":"F538*(1-Elteq!$F$8)","v":7.4067517511414405}]
["REIKU-B","PAIRB-48M50",null,null,10,13.381187397096991,{"$f":"F539*(1-Elteq!$F$8)","v":13.381187397096991}]
["REIKU-B","PAIRB-48P48",null,null,10,13.381187397096991,{"$f":"F540*(1-Elteq!$F$8)","v":13.381187397096991}]
["REIKU-B","PAKGB-36",null,null,10,6.1421843789953412,{"$f":"F541*(1-Elteq!$F$8)","v":6.1421843789953412}]
["REIKU-B","PAKGB-52",null,null,10,6.3873556042073378,{"$f":"F542*(1-Elteq!$F$8)","v":6.3873556042073378}]
["REIKU-B","PAKKB-70",null,null,10,6.4518743476841784,{"$f":"F543*(1-Elteq!$F$8)","v":6.4518743476841784}]
["REIKU-B","PAKMB-17F/G",null,null,25,3.0434954538438563,{"$f":"F544*(1-Elteq!$F$8)","v":3.0434954538438563}]
["REIKU-B","PAKMB-36/36",null,null,10,3.2068938523516435,{"$f":"F545*(1-Elteq!$F$8)","v":3.2068938523516435}]
["REIKU-B","PAKMB-68",null,null,10,6.0884260237892001,{"$f":"F546*(1-Elteq!$F$8)","v":6.0884260237892001}]
["REIKU-B","PAKMB-68/70",null,null,10,6.0883653895055758,{"$f":"F547*(1-Elteq!$F$8)","v":6.0883653895055758}]
["REIKU-B","PAKMB-70",null,null,10,5.3094269078669605,{"$f":"F548*(1-Elteq!$F$8)","v":5.3094269078669605}]
["REIKU-B","PAKMB-90",null,null,10,9.9124706697451952,{"$f":"F549*(1-Elteq!$F$8)","v":9.9124706697451952}]
["REIKU-B","PAKOB-M12",null,null,50,0.77422492172210156,{"$f":"F550*(1-Elteq!$F$8)","v":0.77422492172210156}]
["REIKU-B","PAKOB-M16",null,null,50,1.3677973617090466,{"$f":"F551*(1-Elteq!$F$8)","v":1.3677973617090466}]
["REIKU-B","PAKOB-M20",null,null,50,1.9097548069145172,{"$f":"F552*(1-Elteq!$F$8)","v":1.9097548069145172}]
["REIKU-B","PAKOB-M25",null,null,50,2.0129847964774643,{"$f":"F553*(1-Elteq!$F$8)","v":2.0129847964774643}]
["REIKU-B","PAKOB-M32",null,null,25,3.3162634147096686,{"$f":"F554*(1-Elteq!$F$8)","v":3.3162634147096686}]
["REIKU-B","PAKOB-M40",null,null,10,11.948871291911102,{"$f":"F555*(1-Elteq!$F$8)","v":11.948871291911102}]
["REIKU-B","PAKOB-M50",null,null,5,20.000810477820959,{"$f":"F556*(1-Elteq!$F$8)","v":20.000810477820959}]
["REIKU-B","PAKOB-M63",null,null,5,22.504137724722426,{"$f":"F557*(1-Elteq!$F$8)","v":22.504137724722426}]
["REIKU-B","PAKOB-P07",null,null,50,0.63228368607304952,{"$f":"F558*(1-Elteq!$F$8)","v":0.63228368607304952}]
["REIKU-B","PAKOB-P09",null,null,50,0.64518743476841811,{"$f":"F559*(1-Elteq!$F$8)","v":0.64518743476841811}]
["REIKU-B","PAKOB-P11",null,null,50,0.7613211730267333,{"$f":"F560*(1-Elteq!$F$8)","v":0.7613211730267333}]
["REIKU-B","PAKOB-P13",null,null,50,0.86455116258968001,{"$f":"F561*(1-Elteq!$F$8)","v":0.86455116258968001}]
["REIKU-B","PAKOB-P16",null,null,50,0.9290699060665214,{"$f":"F562*(1-Elteq!$F$8)","v":0.9290699060665214}]
["REIKU-B","PAKOB-P21",null,null,50,1.3548936130136779,{"$f":"F563*(1-Elteq!$F$8)","v":1.3548936130136779}]
["REIKU-B","PAKOB-P29",null,null,25,2.6581722312458824,{"$f":"F564*(1-Elteq!$F$8)","v":2.6581722312458824}]
["REIKU-B","PAKOB-P36",null,null,10,9.6520040241355325,{"$f":"F565*(1-Elteq!$F$8)","v":9.6520040241355325}]
["REIKU-B","PAKOB-P48",null,null,5,17.781365702217595,{"$f":"F566*(1-Elteq!$F$8)","v":17.781365702217595}]
["REIKU-B","PAKPB-29",null,null,10,6.2014106283886079,{"$f":"F567*(1-Elteq!$F$8)","v":6.2014106283886079}]
["REIKU-B","PAKPB-42",null,null,10,11.120913224141814,{"$f":"F568*(1-Elteq!$F$8)","v":11.120913224141814}]
["REIKU-B","PAKTB-70",null,null,10,9.5675872879762611,{"$f":"F569*(1-Elteq!$F$8)","v":9.5675872879762611}]
["REIKU-B","PAM1216",null,null,50,0.74841742433136493,{"$f":"F570*(1-Elteq!$F$8)","v":0.74841742433136493}]
["REIKU-B","PAM1612",null,null,50,0.69680242954989124,{"$f":"F571*(1-Elteq!$F$8)","v":0.69680242954989124}]
["REIKU-B","PAM1620",null,null,50,0.82583991650357502,{"$f":"F572*(1-Elteq!$F$8)","v":0.82583991650357502}]
["REIKU-B","PAM2012",null,null,50,0.78712867041746981,{"$f":"F573*(1-Elteq!$F$8)","v":0.78712867041746981}]
["REIKU-B","PAM2016",null,null,50,0.73551367563599668,{"$f":"F574*(1-Elteq!$F$8)","v":0.73551367563599668}]
["REIKU-B","PAM2025",null,null,50,0.99358864954336401,{"$f":"F575*(1-Elteq!$F$8)","v":0.99358864954336401}]
["REIKU-B","PAM2516",null,null,50,0.3730736362776339,{"$f":"F576*(1-Elteq!$F$8)","v":0.3730736362776339}]
["REIKU-B","PAM2520",null,null,50,1.4968348486627299,{"$f":"F577*(1-Elteq!$F$8)","v":1.4968348486627299}]
["REIKU-B","PAM2532",null,null,25,3.1485146816698792,{"$f":"F578*(1-Elteq!$F$8)","v":3.1485146816698792}]
["REIKU-B","PAM3220",null,null,50,2.9291509538486182,{"$f":"F579*(1-Elteq!$F$8)","v":2.9291509538486182}]
["REIKU-B","PAM3225",null,null,50,2.8001134668949357,{"$f":"F580*(1-Elteq!$F$8)","v":2.8001134668949357}]
["REIKU-B","PAM3240",null,null,25,4.8776170068492419,{"$f":"F581*(1-Elteq!$F$8)","v":4.8776170068492419}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"PAM4025",null,null,25,5.0711732372797664,{"$f":"F582*(1-Elteq!$F$8)","v":5.0711732372797664}]
["REIKU-B","PAM4032",null,null,25,4.9421357503260825,{"$f":"F583*(1-Elteq!$F$8)","v":4.9421357503260825}]
["REIKU-B","PAM5032",null,null,25,6.684141824200811,{"$f":"F584*(1-Elteq!$F$8)","v":6.684141824200811}]
["REIKU-B","PAM5040",null,null,25,6.503489342465655,{"$f":"F585*(1-Elteq!$F$8)","v":6.503489342465655}]
["REIKU-B","PAM6340",null,null,10,8.3358216572079602,{"$f":"F586*(1-Elteq!$F$8)","v":8.3358216572079602}]
["REIKU-B","PAM6350",null,null,10,8.1164579293866996,{"$f":"F587*(1-Elteq!$F$8)","v":8.1164579293866996}]
["REIKU-B","PAMBB-23F/G",null,null,25,3.2259371738420892,{"$f":"F588*(1-Elteq!$F$8)","v":3.2259371738420892}]
["REIKU-B","PAMBB-29F/G",null,null,25,3.2259371738420892,{"$f":"F589*(1-Elteq!$F$8)","v":3.2259371738420892}]
["REIKU-B","PAMBB-36F/G",null,"Leoni",10,1.7671909086835291,{"$f":"F590*(1-Elteq!$F$8)","v":1.7671909086835291}]
["REIKU-B","PAMBB-42",null,null,10,3.3677907253676431,{"$f":"F591*(1-Elteq!$F$8)","v":3.3677907253676431}]
["REIKU-B","PAMBB-42/36",null,null,10,3.3678103294054567,{"$f":"F592*(1-Elteq!$F$8)","v":3.3678103294054567}]
["REIKU-B","PAMBB-48F/G",null,"Leoni",10,2.2580772722067319,{"$f":"F593*(1-Elteq!$F$8)","v":2.2580772722067319}]
["REIKU-B","PAMBB-52",null,"Leoni",10,2.2580772722067319,{"$f":"F594*(1-Elteq!$F$8)","v":2.2580772722067319}]
["REIKU-B","PAMBB-70",null,null,10,4.2475415262935678,{"$f":"F595*(1-Elteq!$F$8)","v":4.2475415262935678}]
["REIKU-B","PAMBB-70L",null,null,10,4.1550070799086116,{"$f":"F596*(1-Elteq!$F$8)","v":4.1550070799086116}]
["REIKU-B","PAMCN-29",null,null,25,1.13885636337383,{"$f":"F597*(1-Elteq!$F$8)","v":1.13885636337383}]
["REIKU-B","PAMCN-36",null,null,25,1.13885636337383,{"$f":"F598*(1-Elteq!$F$8)","v":1.13885636337383}]
["REIKU-B","PAMCN-42",null,null,25,1.13885636337383,{"$f":"F599*(1-Elteq!$F$8)","v":1.13885636337383}]
["REIKU-B","PAMCN-52",null,null,25,1.13885636337383,{"$f":"F600*(1-Elteq!$F$8)","v":1.13885636337383}]
["REIKU-B","PAMCN-70",null,null,25,1.13885636337383,{"$f":"F601*(1-Elteq!$F$8)","v":1.13885636337383}]
["REIKU-B","PANOB-07M081",null,null,50,2.2581560216894632,{"$f":"F602*(1-Elteq!$F$8)","v":2.2581560216894632}]
["REIKU-B","PANOB-07M121",null,null,50,2.2581560216894632,{"$f":"F603*(1-Elteq!$F$8)","v":2.2581560216894632}]
["REIKU-B","PANOB-07M181",null,null,50,2.2581560216894632,{"$f":"F604*(1-Elteq!$F$8)","v":2.2581560216894632}]
["REIKU-B","PANOB-07M301",null,null,50,2.5678459903783031,{"$f":"F605*(1-Elteq!$F$8)","v":2.5678459903783031}]
["REIKU-B","PANOB-10M081",null,null,50,2.2581560216894632,{"$f":"F606*(1-Elteq!$F$8)","v":2.2581560216894632}]
["REIKU-B","PANOB-10M121",null,null,50,2.2581560216894632,{"$f":"F607*(1-Elteq!$F$8)","v":2.2581560216894632}]
["REIKU-B","PANOB-10M181",null,null,50,2.2581560216894632,{"$f":"F608*(1-Elteq!$F$8)","v":2.2581560216894632}]
["REIKU-B","PANOB-10M301",null,null,50,2.5678459903783031,{"$f":"F609*(1-Elteq!$F$8)","v":2.5678459903783031}]
["REIKU-B","PAP1109",null,null,100,1.0839148904109424,{"$f":"F610*(1-Elteq!$F$8)","v":1.0839148904109424}]
["REIKU-B","PAP1113",null,null,100,0.79955570890659233,{"$f":"F611*(1-Elteq!$F$8)","v":0.79955570890659233}]
["REIKU-B","PAP1309",null,null,100,0.83874366519894328,{"$f":"F612*(1-Elteq!$F$8)","v":0.83874366519894328}]
["REIKU-B","PAP1311",null,null,100,1.0581073930202056,{"$f":"F613*(1-Elteq!$F$8)","v":1.0581073930202056}]
["REIKU-B","PAP1316",null,null,100,0.61507668640366475,{"$f":"F614*(1-Elteq!$F$8)","v":0.61507668640366475}]
["REIKU-B","PAP1609",null,null,100,0.85164741389431153,{"$f":"F615*(1-Elteq!$F$8)","v":0.85164741389431153}]
["REIKU-B","PAP1611",null,null,100,0.78712867041746981,{"$f":"F616*(1-Elteq!$F$8)","v":0.78712867041746981}]
["REIKU-B","PAP1613",null,null,100,1.1226261364970476,{"$f":"F617*(1-Elteq!$F$8)","v":1.1226261364970476}]
["REIKU-B","PAP2113",null,null,100,2.1162147860404112,{"$f":"F618*(1-Elteq!$F$8)","v":2.1162147860404112}]
["REIKU-B","PAP2116",null,null,100,1.8194285660469385,{"$f":"F619*(1-Elteq!$F$8)","v":1.8194285660469385}]
["REIKU-B","PAP2921",null,null,50,3.3678784094911429,{"$f":"F620*(1-Elteq!$F$8)","v":3.3678784094911429}]
["REIKU-B","PAP3629",null,null,25,5.7421681694389211,{"$f":"F621*(1-Elteq!$F$8)","v":5.7421681694389211}]
["REIKU-B","PAPKB-17F/G",null,null,25,3.5049286355556664,{"$f":"F622*(1-Elteq!$F$8)","v":3.5049286355556664}]
["REIKU-B","PAPKB-29F/G",null,null,25,6.5163148620649594,{"$f":"F623*(1-Elteq!$F$8)","v":6.5163148620649594}]
["REIKU-B","PAPKB-36F/G",null,null,10,7.4971613988581964,{"$f":"F624*(1-Elteq!$F$8)","v":7.4971613988581964}]
["REIKU-B","PAPRB-23F/G",null,null,25,5.4066707033593433,{"$f":"F625*(1-Elteq!$F$8)","v":5.4066707033593433}]
["REIKU-B","PAPRB-29F/G",null,null,25,6.5163930911610208,{"$f":"F626*(1-Elteq!$F$8)","v":6.5163930911610208}]
["REIKU-B","PAPRB-36F/G",null,null,10,7.4970779920090189,{"$f":"F627*(1-Elteq!$F$8)","v":7.4970779920090189}]
["REIKU-B","PAPRB-42",null,null,10,8.0853991772930662,{"$f":"F628*(1-Elteq!$F$8)","v":8.0853991772930662}]
["REIKU-B","PAPRB-48F/G",null,null,10,8.0648429346052239,{"$f":"F629*(1-Elteq!$F$8)","v":8.0648429346052239}]
["REIKU-B","PAPRB-52",null,null,10,9.1100465789300618,{"$f":"F630*(1-Elteq!$F$8)","v":9.1100465789300618}]
["REIKU-B","PAPRB-52BL",null,null,10,9.1100465789300618,{"$f":"F631*(1-Elteq!$F$8)","v":9.1100465789300618}]
["REIKU-B","PAPRB-68",null,null,10,12.66531932310216,{"$f":"F632*(1-Elteq!$F$8)","v":12.66531932310216}]
["REIKU-B","PAPRB-70",null,null,10,11.680739197307316,{"$f":"F633*(1-Elteq!$F$8)","v":11.680739197307316}]
["REIKU-B","PAPRB-70BL",null,null,10,12.530247502566024,{"$f":"F634*(1-Elteq!$F$8)","v":12.530247502566024}]
["REIKU-B","PAPRB-90",null,null,10,14.589332455808883,{"$f":"F635*(1-Elteq!$F$8)","v":14.589332455808883}]
["REIKU-B","PARAB-07G",null,null,100,1.0844661542954592,{"$f":"F636*(1-Elteq!$F$8)","v":1.0844661542954592}]
["REIKU-B","PARAB–10F",null,null,100,1.1028344003134387,{"$f":"F637*(1-Elteq!$F$8)","v":1.1028344003134387}]
["REIKU-B","PARAB–12F",null,null,50,1.5049094420943803,{"$f":"F638*(1-Elteq!$F$8)","v":1.5049094420943803}]
["REIKU-B","PARAB–17F",null,null,50,2.320547383992861,{"$f":"F639*(1-Elteq!$F$8)","v":2.320547383992861}]
["REIKU-B","PARAB–23F",null,null,50,3.7105782427212577,{"$f":"F640*(1-Elteq!$F$8)","v":3.7105782427212577}]
["REIKU-B","PARAB-23G",null,null,50,3.7318159503527246,{"$f":"F641*(1-Elteq!$F$8)","v":3.7318159503527246}]
["REIKU-B","PARAB–29F",null,null,50,4.698534059668714,{"$f":"F642*(1-Elteq!$F$8)","v":4.698534059668714}]
["REIKU-B","PARAB–29G",null,null,50,4.698534059668714,{"$f":"F643*(1-Elteq!$F$8)","v":4.698534059668714}]
["REIKU-B","PARAB-36F",null,null,30,6.6629578352270276,{"$f":"F644*(1-Elteq!$F$8)","v":6.6629578352270276}]
["REIKU-B","PARAB–36G",null,null,30,6.6629578352270276,{"$f":"F645*(1-Elteq!$F$8)","v":6.6629578352270276}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"PARAB-42M",null,null,30,6.9623576928241002,{"$f":"F646*(1-Elteq!$F$8)","v":6.9623576928241002}]
["REIKU-B","PARAB-48F",null,null,30,9.2362381026250517,{"$f":"F647*(1-Elteq!$F$8)","v":9.2362381026250517}]
["REIKU-B","PARAB-48G",null,null,30,9.2362381026250517,{"$f":"F648*(1-Elteq!$F$8)","v":9.2362381026250517}]
["REIKU-B","PARAB-52G",null,null,30,13.211037087088064,{"$f":"F649*(1-Elteq!$F$8)","v":13.211037087088064}]
["REIKU-B","PARAB-68G",null,null,30,20.595266975615932,{"$f":"F650*(1-Elteq!$F$8)","v":20.595266975615932}]
["REIKU-B","PARAB-70G",null,null,"10/30",21.81544298120021,{"$f":"F651*(1-Elteq!$F$8)","v":21.81544298120021}]
["REIKU-B","PARBB-12F",null,null,50,1.2713956815250946,{"$f":"F652*(1-Elteq!$F$8)","v":1.2713956815250946}]
["REIKU-B","PARBB-17F",null,null,50,2.1304468176906992,{"$f":"F653*(1-Elteq!$F$8)","v":2.1304468176906992}]
["REIKU-B","PARBB-23F",null,null,50,3.3674804537691694,{"$f":"F654*(1-Elteq!$F$8)","v":3.3674804537691694}]
["REIKU-B","PARBB-29F",null,null,50,3.8622939082005572,{"$f":"F655*(1-Elteq!$F$8)","v":3.8622939082005572}]
["REIKU-B","PARBB-36G",null,null,30,5.9308890440873325,{"$f":"F656*(1-Elteq!$F$8)","v":5.9308890440873325}]
["REIKU-B","PARBB-48G",null,null,30,8.3568494526190022,{"$f":"F657*(1-Elteq!$F$8)","v":8.3568494526190022}]
["REIKU-B","PAREB–07G",null,null,100,0.53015727260505874,{"$f":"F658*(1-Elteq!$F$8)","v":0.53015727260505874}]
["REIKU-B","PAREB–10F",null,null,100,0.55764690896235813,{"$f":"F659*(1-Elteq!$F$8)","v":0.55764690896235813}]
["REIKU-B","PAREB–12F",null,null,50,0.69902218165704055,{"$f":"F660*(1-Elteq!$F$8)","v":0.69902218165704055}]
["REIKU-B","PAREB–14F",null,null,50,0.92286636342362072,{"$f":"F661*(1-Elteq!$F$8)","v":0.92286636342362072}]
["REIKU-B","PAREB–17F",null,null,50,0.98550346340918149,{"$f":"F662*(1-Elteq!$F$8)","v":0.98550346340918149}]
["REIKU-B","PAREB–23F",null,null,50,1.771117999591715,{"$f":"F663*(1-Elteq!$F$8)","v":1.771117999591715}]
["REIKU-B","PAREB–29F",null,null,30,2.1284832722366067,{"$f":"F664*(1-Elteq!$F$8)","v":2.1284832722366067}]
["REIKU-B","PAREB–36F",null,null,30,3.1632717265435177,{"$f":"F665*(1-Elteq!$F$8)","v":3.1632717265435177}]
["REIKU-B","PAREB–48F",null,null,30,4.4788471807857011,{"$f":"F666*(1-Elteq!$F$8)","v":4.4788471807857011}]
["REIKU-B","PAREB–52G",null,null,"10/30",6.5346792712208721,{"$f":"F667*(1-Elteq!$F$8)","v":6.5346792712208721}]
["REIKU-B","PAREB–70G",null,null,"10/30",11.742001815475005,{"$f":"F668*(1-Elteq!$F$8)","v":11.742001815475005}]
["REIKU-B","PAREB–95G",null,null,"10/30",15.943989087233621,{"$f":"F669*(1-Elteq!$F$8)","v":15.943989087233621}]
["REIKU-B","PARFB-10F",null,null,100,3.4905742677170633,{"$f":"F670*(1-Elteq!$F$8)","v":3.4905742677170633}]
["REIKU-B","PARFB-12F",null,null,50,3.5545041993602342,{"$f":"F671*(1-Elteq!$F$8)","v":3.5545041993602342}]
["REIKU-B","PARFB-17F",null,null,50,5.7920518068711697,{"$f":"F672*(1-Elteq!$F$8)","v":5.7920518068711697}]
["REIKU-B","PARFB-17G",null,null,50,5.7920518068711697,{"$f":"F673*(1-Elteq!$F$8)","v":5.7920518068711697}]
["REIKU-B","PARFB-23G",null,null,50,8.2213892093116208,{"$f":"F674*(1-Elteq!$F$8)","v":8.2213892093116208}]
["REIKU-B","PARFB-29G",null,null,50,9.4232719242032097,{"$f":"F675*(1-Elteq!$F$8)","v":9.4232719242032097}]
["REIKU-B","PARFB-36G",null,null,30,12.952204150906175,{"$f":"F676*(1-Elteq!$F$8)","v":12.952204150906175}]
["REIKU-B","PARFB-48G",null,null,30,16.123128760407393,{"$f":"F677*(1-Elteq!$F$8)","v":16.123128760407393}]
["REIKU-B","PARFB-52G",null,null,30,22.580051856367536,{"$f":"F678*(1-Elteq!$F$8)","v":22.580051856367536}]
["REIKU-B","PARFB-70G",null,null,"10/30",37.002644435066593,{"$f":"F679*(1-Elteq!$F$8)","v":37.002644435066593}]
["REIKU-B","PARGB-48",null,null,10,4.0001620955641917,{"$f":"F680*(1-Elteq!$F$8)","v":4.0001620955641917}]
["REIKU-B","PARGB-48T",null,null,10,7.5393862091710826,{"$f":"F681*(1-Elteq!$F$8)","v":7.5393862091710826}]
["REIKU-B","PARGB-48L48K",null,null,10,3.2726828294932355,{"$f":"F682*(1-Elteq!$F$8)","v":3.2726828294932355}]
["REIKU-B","PARGB-48L52K",null,null,10,3.2726828294932355,{"$f":"F683*(1-Elteq!$F$8)","v":3.2726828294932355}]
["REIKU-B","PARGB-48R48K",null,null,10,3.2726828294932355,{"$f":"F684*(1-Elteq!$F$8)","v":3.2726828294932355}]
["REIKU-B","PARGB-48R52K",null,null,10,3.2726828294932355,{"$f":"F685*(1-Elteq!$F$8)","v":3.2726828294932355}]
["REIKU-B","PARGB-76",null,null,10,10.434298136416462,{"$f":"F686*(1-Elteq!$F$8)","v":10.434298136416462}]
["REIKU-B","PARGB-76L70",null,null,10,7.99960733354499,{"$f":"F687*(1-Elteq!$F$8)","v":7.99960733354499}]
["REIKU-B","PARGB-76L90",null,null,10,7.99960733354499,{"$f":"F688*(1-Elteq!$F$8)","v":7.99960733354499}]
["REIKU-B","PARGB-76R70",null,null,10,7.99960733354499,{"$f":"F689*(1-Elteq!$F$8)","v":7.99960733354499}]
["REIKU-B","PARGB-76R90",null,null,10,7.99960733354499,{"$f":"F690*(1-Elteq!$F$8)","v":7.99960733354499}]
["REIKU-B","PARNB–07G",null,null,100,0.98713677519567966,{"$f":"F691*(1-Elteq!$F$8)","v":0.98713677519567966}]
["REIKU-B","PARNB–10F",null,null,100,1.0103635228473427,{"$f":"F692*(1-Elteq!$F$8)","v":1.0103635228473427}]
["REIKU-B","PARNB–12F",null,null,50,1.3355379899706257,{"$f":"F693*(1-Elteq!$F$8)","v":1.3355379899706257}]
["REIKU-B","PARNB–14F",null,null,50,1.776846195352223,{"$f":"F694*(1-Elteq!$F$8)","v":1.776846195352223}]
["REIKU-B","PARNB–17F",null,null,50,2.2413811483854844,{"$f":"F695*(1-Elteq!$F$8)","v":2.2413811483854844}]
["REIKU-B","PARNB–17G",null,null,50,2.2413811483854844,{"$f":"F696*(1-Elteq!$F$8)","v":2.2413811483854844}]
["REIKU-B","PARNB–23F",null,null,50,3.5420790168786143,{"$f":"F697*(1-Elteq!$F$8)","v":3.5420790168786143}]
["REIKU-B","PARNB–23G",null,null,50,3.5420790168786143,{"$f":"F698*(1-Elteq!$F$8)","v":3.5420790168786143}]
["REIKU-B","PARNB–29F",null,null,50,4.0646808390410332,{"$f":"F699*(1-Elteq!$F$8)","v":4.0646808390410332}]
["REIKU-B","PARNB–29G",null,null,50,4.0646808390410332,{"$f":"F700*(1-Elteq!$F$8)","v":4.0646808390410332}]
["REIKU-B","PARNB–36F",null,null,30,6.2479951182973608,{"$f":"F701*(1-Elteq!$F$8)","v":6.2479951182973608}]
["REIKU-B","PARNB–36G",null,null,30,6.2479951182973608,{"$f":"F702*(1-Elteq!$F$8)","v":6.2479951182973608}]
["REIKU-B","PARNB–48F",null,null,30,8.8029373599802963,{"$f":"F703*(1-Elteq!$F$8)","v":8.8029373599802963}]
["REIKU-B","PARNB–48G",null,null,30,8.8029373599802963,{"$f":"F704*(1-Elteq!$F$8)","v":8.8029373599802963}]
["REIKU-B","PARNB–52G",null,null,"10/30",10.03395498551844,{"$f":"F705*(1-Elteq!$F$8)","v":10.03395498551844}]
["REIKU-B","PARNB–70G",null,null,"10/30",16.363243720596618,{"$f":"F706*(1-Elteq!$F$8)","v":16.363243720596618}]
["REIKU-B","PARNB–95G",null,null,"10/30",21.949276530821589,{"$f":"F707*(1-Elteq!$F$8)","v":21.949276530821589}]
["REIKU-B","PARRB–07G",null,null,100,1.4192444824783663,{"$f":"F708*(1-Elteq!$F$8)","v":1.4192444824783663}]
["REIKU-B","PARRB–10F",null,null,100,1.4576024414642688,{"$f":"F709*(1-Elteq!$F$8)","v":1.4576024414642688}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"PARRB–12F",null,null,50,2.0073998535955275,{"$f":"F710*(1-Elteq!$F$8)","v":2.0073998535955275}]
["REIKU-B","PARRB–17F",null,null,50,3.119780664186679,{"$f":"F711*(1-Elteq!$F$8)","v":3.119780664186679}]
["REIKU-B","PARRB–23F",null,null,50,4.9226047365240655,{"$f":"F712*(1-Elteq!$F$8)","v":4.9226047365240655}]
["REIKU-B","PARRB–23G",null,null,50,4.9226047365240655,{"$f":"F713*(1-Elteq!$F$8)","v":4.9226047365240655}]
["REIKU-B","PARRB–29F",null,null,50,6.239561328373358,{"$f":"F714*(1-Elteq!$F$8)","v":6.239561328373358}]
["REIKU-B","PARRB–29G",null,null,50,6.239561328373358,{"$f":"F715*(1-Elteq!$F$8)","v":6.239561328373358}]
["REIKU-B","PARRB-36F",null,null,30,8.8479321706876117,{"$f":"F716*(1-Elteq!$F$8)","v":8.8479321706876117}]
["REIKU-B","PARRB–36G",null,null,30,8.8479025394146813,{"$f":"F717*(1-Elteq!$F$8)","v":8.8479025394146813}]
["REIKU-B","PARRB-48F",null,null,30,12.798781978867757,{"$f":"F718*(1-Elteq!$F$8)","v":12.798781978867757}]
["REIKU-B","PARRB–48G",null,null,30,12.798772314962568,{"$f":"F719*(1-Elteq!$F$8)","v":12.798772314962568}]
["REIKU-B","PARRB–52G",null,null,30,18.565252149176473,{"$f":"F720*(1-Elteq!$F$8)","v":18.565252149176473}]
["REIKU-B","PARRB–70G",null,null,"10/30",30.238857667219246,{"$f":"F721*(1-Elteq!$F$8)","v":30.238857667219246}]
["REIKU-B","PARRB–95G",null,null,"10/30",35.020816554128345,{"$f":"F722*(1-Elteq!$F$8)","v":35.020816554128345}]
["REIKU-B","PARTB-10",null,"otvoriteľná hadica",50,2.5722445448615816,{"$f":"F723*(1-Elteq!$F$8)","v":2.5722445448615816}]
["REIKU-B","PARTB-12",null,"otvoriteľná hadica",50,3.0434954538438563,{"$f":"F724*(1-Elteq!$F$8)","v":3.0434954538438563}]
["REIKU-B","PARTB-14",null,"otvoriteľná hadica",50,3.2594854537940652,{"$f":"F725*(1-Elteq!$F$8)","v":3.2594854537940652}]
["REIKU-B","PARTB-17",null,"otvoriteľná hadica",50,3.4951109082852021,{"$f":"F726*(1-Elteq!$F$8)","v":3.4951109082852021}]
["REIKU-B","PARTB-24",null,"otvoriteľná hadica",25,5.3015727260505878,{"$f":"F727*(1-Elteq!$F$8)","v":5.3015727260505878}]
["REIKU-B","PARTB-29",null,"otvoriteľná hadica",25,7.6391735891480774,{"$f":"F728*(1-Elteq!$F$8)","v":7.6391735891480774}]
["REIKU-B","PARTB-34",null,"otvoriteľná hadica",25,9.7884704431980705,{"$f":"F729*(1-Elteq!$F$8)","v":9.7884704431980705}]
["REIKU-B","PARTB-45",null,"otvoriteľná hadica",25,11.540542051885081,{"$f":"F730*(1-Elteq!$F$8)","v":11.540542051885081}]
["REIKU-B","PARTB-68",null,"otvoriteľná hadica",10,29.3186789477868,{"$f":"F731*(1-Elteq!$F$8)","v":29.3186789477868}]
["REIKU-B","PARVB–07G",null,null,100,1.4400583544031094,{"$f":"F732*(1-Elteq!$F$8)","v":1.4400583544031094}]
["REIKU-B","PARVB–10F",null,null,100,1.4516717282289404,{"$f":"F733*(1-Elteq!$F$8)","v":1.4516717282289404}]
["REIKU-B","PARVB–12F",null,null,50,1.9162066812622018,{"$f":"F734*(1-Elteq!$F$8)","v":1.9162066812622018}]
["REIKU-B","PARVB–17F",null,null,50,3.658212755136931,{"$f":"F735*(1-Elteq!$F$8)","v":3.658212755136931}]
["REIKU-B","PARVB–17G",null,null,50,3.658212755136931,{"$f":"F736*(1-Elteq!$F$8)","v":3.658212755136931}]
["REIKU-B","PARVB–23F",null,null,50,5.5163525672699754,{"$f":"F737*(1-Elteq!$F$8)","v":5.5163525672699754}]
["REIKU-B","PARVB–23G",null,null,50,5.5163525672699754,{"$f":"F738*(1-Elteq!$F$8)","v":5.5163525672699754}]
["REIKU-B","PARVB–29F",null,null,50,6.4338090995106674,{"$f":"F739*(1-Elteq!$F$8)","v":6.4338090995106674}]
["REIKU-B","PARVB–29G",null,null,50,6.4338090995106674,{"$f":"F740*(1-Elteq!$F$8)","v":6.4338090995106674}]
["REIKU-B","PARVB–36G",null,null,30,10.289449209686733,{"$f":"F741*(1-Elteq!$F$8)","v":10.289449209686733}]
["REIKU-B","PARVB–48G",null,null,30,12.286949507729748,{"$f":"F742*(1-Elteq!$F$8)","v":12.286949507729748}]
["REIKU-B","PARVB–52G",null,null,"10/30",17.780075327348069,{"$f":"F743*(1-Elteq!$F$8)","v":17.780075327348069}]
["REIKU-B","PARVB–70G",null,null,"10/30",28.998594443101318,{"$f":"F744*(1-Elteq!$F$8)","v":28.998594443101318}]
["REIKU-B","PARVB–95G",null,null,"10/30",34.665920870107094,{"$f":"F745*(1-Elteq!$F$8)","v":34.665920870107094}]
["REIKU-B","PASOB-07M12",null,null,50,2.4259047547292516,{"$f":"F746*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-B","PASOB-07M12",null,null,50,2.4259047547292516,{"$f":"F747*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-B","PASOB-07M16",null,null,50,2.4259047547292516,{"$f":"F748*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-B","PASOB-07M16",null,null,50,2.4259047547292516,{"$f":"F749*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-B","PASOB-07M20",null,null,50,2.4259047547292516,{"$f":"F750*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-B","PASOB-07M20",null,null,50,2.4259047547292516,{"$f":"F751*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-B","PASOB-07P07",null,null,50,2.4259047547292516,{"$f":"F752*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-B","PASOB-07P09",null,null,50,2.4259047547292516,{"$f":"F753*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-B","PASOB-07P11",null,null,50,2.4259047547292516,{"$f":"F754*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-B","PASOB-07P13",null,null,50,2.4259047547292516,{"$f":"F755*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-B","PASOB-17M25",null,null,50,3.1743221790606166,{"$f":"F756*(1-Elteq!$F$8)","v":3.1743221790606166}]
["REIKU-B","PASOB-17P16",null,null,50,3.1743221790606166,{"$f":"F757*(1-Elteq!$F$8)","v":3.1743221790606166}]
["REIKU-B","PASOB-23M32",null,null,30,4.6969645251140832,{"$f":"F758*(1-Elteq!$F$8)","v":4.6969645251140832}]
["REIKU-B","PASOB-23P21",null,null,30,4.6969645251140832,{"$f":"F759*(1-Elteq!$F$8)","v":4.6969645251140832}]
["REIKU-B","PASOB-52",null,null,10,24.804487948827429,{"$f":"F760*(1-Elteq!$F$8)","v":24.804487948827429}]
["REIKU-B","PASOB-70",null,null,10,33.652976597520684,{"$f":"F761*(1-Elteq!$F$8)","v":33.652976597520684}]
["REIKU-B","PASOB-95",null,null,10,42.879156914709057,{"$f":"F762*(1-Elteq!$F$8)","v":42.879156914709057}]
["REIKU-B","PASSB-17K",null,null,25,6.3127986349083844,{"$f":"F763*(1-Elteq!$F$8)","v":6.3127986349083844}]
["REIKU-B","PASSB-29K",null,null,25,9.3036028093605871,{"$f":"F764*(1-Elteq!$F$8)","v":9.3036028093605871}]
["REIKU-B","PASSB-36K",null,null,10,10.268431639814699,{"$f":"F765*(1-Elteq!$F$8)","v":10.268431639814699}]
["REIKU-B","PASSB-36S",null,null,10,10.884325161127268,{"$f":"F766*(1-Elteq!$F$8)","v":10.884325161127268}]
["REIKU-B","PASSB-52K",null,null,10,14.503813533594043,{"$f":"F767*(1-Elteq!$F$8)","v":14.503813533594043}]
["REIKU-B","PASSB-52M",null,null,10,22.775116447325164,{"$f":"F768*(1-Elteq!$F$8)","v":22.775116447325164}]
["REIKU-B","PASSB-52S",null,null,10,17.671909086835292,{"$f":"F769*(1-Elteq!$F$8)","v":17.671909086835292}]
["REIKU-B","PASSB-70K",null,null,10,16.990166105174271,{"$f":"F770*(1-Elteq!$F$8)","v":16.990166105174271}]
["REIKU-B","PASSB-70M",null,null,10,23.149101318299948,{"$f":"F771*(1-Elteq!$F$8)","v":23.149101318299948}]
["REIKU-B","PASSB-70SE",null,null,10,24.022183479029582,{"$f":"F772*(1-Elteq!$F$8)","v":24.022183479029582}]
["REIKU-B","PASVB-07M12",null,null,50,2.7614022208088285,{"$f":"F773*(1-Elteq!$F$8)","v":2.7614022208088285}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"PASVB-07M12",null,null,50,2.7614022208088285,{"$f":"F774*(1-Elteq!$F$8)","v":2.7614022208088285}]
["REIKU-B","PASVB-07M16",null,null,50,2.7743059695041974,{"$f":"F775*(1-Elteq!$F$8)","v":2.7743059695041974}]
["REIKU-B","PASVB-07M16",null,null,50,2.7743059695041974,{"$f":"F776*(1-Elteq!$F$8)","v":2.7743059695041974}]
["REIKU-B","PASVB-07M20",null,null,50,2.8130172155903033,{"$f":"F777*(1-Elteq!$F$8)","v":2.8130172155903033}]
["REIKU-B","PASVB-07M20",null,null,50,2.8130172155903033,{"$f":"F778*(1-Elteq!$F$8)","v":2.8130172155903033}]
["REIKU-B","PASVB-07P07",null,null,50,2.7614022208088285,{"$f":"F779*(1-Elteq!$F$8)","v":2.7614022208088285}]
["REIKU-B","PASVB-07P09",null,null,50,2.7614022208088285,{"$f":"F780*(1-Elteq!$F$8)","v":2.7614022208088285}]
["REIKU-B","PASVB-07P11",null,null,50,2.7743059695041974,{"$f":"F781*(1-Elteq!$F$8)","v":2.7743059695041974}]
["REIKU-B","PASVB-07P13",null,null,50,2.787209718199565,{"$f":"F782*(1-Elteq!$F$8)","v":2.787209718199565}]
["REIKU-B","PASVB-17M25",null,null,50,3.638857132093877,{"$f":"F783*(1-Elteq!$F$8)","v":3.638857132093877}]
["REIKU-B","PASVB-17P16",null,null,50,3.6001458860077729,{"$f":"F784*(1-Elteq!$F$8)","v":3.6001458860077729}]
["REIKU-B","PASVB-23M32",null,null,30,5.4324782007500803,{"$f":"F785*(1-Elteq!$F$8)","v":5.4324782007500803}]
["REIKU-B","PASVB-23P21",null,null,30,5.3421519598825027,{"$f":"F786*(1-Elteq!$F$8)","v":5.3421519598825027}]
["REIKU-B","PATBB-70",null,null,10,11.09722387801679,{"$f":"F787*(1-Elteq!$F$8)","v":11.09722387801679}]
["REIKU-B","PAVGB-23",null,null,10,5.8611831804670373,{"$f":"F788*(1-Elteq!$F$8)","v":5.8611831804670373}]
["REIKU-B","PAVGB-36",null,null,10,7.7560045436666005,{"$f":"F789*(1-Elteq!$F$8)","v":7.7560045436666005}]
["REIKU-B","PAVGB-70",null,null,10,9.5569684341605257,{"$f":"F790*(1-Elteq!$F$8)","v":9.5569684341605257}]
["REIKU-B","PAVSB",null,null,100,7.7422492172210172E-2,{"$f":"F791*(1-Elteq!$F$8)","v":7.7422492172210172E-2}]
["REIKU-B","PAWAB-14/17",null,null,50,0.77422492172210156,{"$f":"F792*(1-Elteq!$F$8)","v":0.77422492172210156}]
["REIKU-B","PAWOB-07P07",null,null,50,2.2065410269079901,{"$f":"F793*(1-Elteq!$F$8)","v":2.2065410269079901}]
["REIKU-B","PAWOB-10M16",null,null,50,2.2194447756033582,{"$f":"F794*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-B","PAWOB-10M20",null,null,50,2.2194447756033582,{"$f":"F795*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-B","PAWOB-10P07",null,null,50,2.2065410269079901,{"$f":"F796*(1-Elteq!$F$8)","v":2.2065410269079901}]
["REIKU-B","PAWOB-10P09",null,null,50,2.2194447756033582,{"$f":"F797*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-B","PAWOB-10P11",null,null,50,2.2194447756033582,{"$f":"F798*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-B","PAWOB-12M16",null,null,50,2.2194447756033582,{"$f":"F799*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-B","PAWOB-12M20",null,null,50,2.2194447756033582,{"$f":"F800*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-B","PAWOB-12P09",null,null,50,2.2194447756033582,{"$f":"F801*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-B","PAWOB-12P11",null,null,50,2.2194447756033582,{"$f":"F802*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-B","PAWOB-12P13",null,null,50,2.2194447756033582,{"$f":"F803*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-B","PAWOB-17M20",null,null,50,1.8820583177479586,{"$f":"F804*(1-Elteq!$F$8)","v":1.8820583177479586}]
["REIKU-B","PAWOB-17M25",null,null,50,2.2323548267581161,{"$f":"F805*(1-Elteq!$F$8)","v":2.2323548267581161}]
["REIKU-B","PAWOB-17P13",null,null,50,2.2323485242987262,{"$f":"F806*(1-Elteq!$F$8)","v":2.2323485242987262}]
["REIKU-B","PAWOB-17P16",null,null,50,2.2323485242987262,{"$f":"F807*(1-Elteq!$F$8)","v":2.2323485242987262}]
["REIKU-B","PAWOB-23M25",null,null,30,3.7162796242660856,{"$f":"F808*(1-Elteq!$F$8)","v":3.7162796242660856}]
["REIKU-B","PAWOB-23P21",null,null,30,3.7162796242660856,{"$f":"F809*(1-Elteq!$F$8)","v":3.7162796242660856}]
["REIKU-B","PAWOB-29M32",null,null,30,5.3292482111871333,{"$f":"F810*(1-Elteq!$F$8)","v":5.3292482111871333}]
["REIKU-B","PAWOB-29P29",null,null,30,5.3292482111871333,{"$f":"F811*(1-Elteq!$F$8)","v":5.3292482111871333}]
["REIKU-B","PAWOB-36M40",null,null,10,8.8003566102412201,{"$f":"F812*(1-Elteq!$F$8)","v":8.8003566102412201}]
["REIKU-B","PAWOB-36P36",null,null,10,8.8003566102412201,{"$f":"F813*(1-Elteq!$F$8)","v":8.8003566102412201}]
["REIKU-B","PAWOB-48M50",null,null,10,9.8326565058706912,{"$f":"F814*(1-Elteq!$F$8)","v":9.8326565058706912}]
["REIKU-B","PAWOB-48P48",null,null,10,9.8326565058706912,{"$f":"F815*(1-Elteq!$F$8)","v":9.8326565058706912}]
["REIKU-B","PAWOB-52",null,null,10,15.75489966000448,{"$f":"F816*(1-Elteq!$F$8)","v":15.75489966000448}]
["REIKU-B","PAWOB-70",null,null,10,22.258966499510418,{"$f":"F817*(1-Elteq!$F$8)","v":22.258966499510418}]
["REIKU-B","PAWOB-95",null,null,10,28.994723318492724,{"$f":"F818*(1-Elteq!$F$8)","v":28.994723318492724}]
["REIKU-B","PAWVB-07P07",null,null,50,2.5549422416829355,{"$f":"F819*(1-Elteq!$F$8)","v":2.5549422416829355}]
["REIKU-B","PAWVB-10M16",null,null,50,2.5936534877690405,{"$f":"F820*(1-Elteq!$F$8)","v":2.5936534877690405}]
["REIKU-B","PAWVB-10M20",null,null,50,2.6323647338551464,{"$f":"F821*(1-Elteq!$F$8)","v":2.6323647338551464}]
["REIKU-B","PAWVB-10P07",null,null,50,2.5678459903783031,{"$f":"F822*(1-Elteq!$F$8)","v":2.5678459903783031}]
["REIKU-B","PAWVB-10P09",null,null,50,2.5807497390736724,{"$f":"F823*(1-Elteq!$F$8)","v":2.5807497390736724}]
["REIKU-B","PAWVB-10P11",null,null,50,2.5936534877690405,{"$f":"F824*(1-Elteq!$F$8)","v":2.5936534877690405}]
["REIKU-B","PAWVB-10P11K",null,null,50,2.5936534877690405,{"$f":"F825*(1-Elteq!$F$8)","v":2.5936534877690405}]
["REIKU-B","PAWVB-10P13",null,null,50,2.6065572364644094,{"$f":"F826*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-B","PAWVB-12M16",null,null,50,2.6065572364644094,{"$f":"F827*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-B","PAWVB-12M20",null,null,50,2.6452684825505144,{"$f":"F828*(1-Elteq!$F$8)","v":2.6452684825505144}]
["REIKU-B","PAWVB-12P09",null,null,50,2.5936534877690405,{"$f":"F829*(1-Elteq!$F$8)","v":2.5936534877690405}]
["REIKU-B","PAWVB-12P11",null,null,50,2.6065572364644094,{"$f":"F830*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-B","PAWVB-12P13",null,null,50,2.6194609851597779,{"$f":"F831*(1-Elteq!$F$8)","v":2.6194609851597779}]
["REIKU-B","PAWVB-17M20",null,null,50,2.6710759799412513,{"$f":"F832*(1-Elteq!$F$8)","v":2.6710759799412513}]
["REIKU-B","PAWVB-17P13",null,null,50,2.6452684825505144,{"$f":"F833*(1-Elteq!$F$8)","v":2.6452684825505144}]
["REIKU-B","PAWVB-17P16",null,null,50,2.6581722312458824,{"$f":"F834*(1-Elteq!$F$8)","v":2.6581722312458824}]
["REIKU-B","PAWVB-23M25",null,null,30,4.3614670590345064,{"$f":"F835*(1-Elteq!$F$8)","v":4.3614670590345064}]
["REIKU-B","PAWVB-23P21",null,null,30,4.3614670590345064,{"$f":"F836*(1-Elteq!$F$8)","v":4.3614670590345064}]
["REIKU-B","PAWVB-29M32",null,null,30,6.1808956250814449,{"$f":"F837*(1-Elteq!$F$8)","v":6.1808956250814449}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"PAWVB-29P29",null,null,30,6.1808956250814449,{"$f":"F838*(1-Elteq!$F$8)","v":6.1808956250814449}]
["REIKU-B","PAWVB-36M40",null,null,10,10.090731479778055,{"$f":"F839*(1-Elteq!$F$8)","v":10.090731479778055}]
["REIKU-B","PAWVB-36P36",null,null,10,9.9875014902151147,{"$f":"F840*(1-Elteq!$F$8)","v":9.9875014902151147}]
["REIKU-B","PAWVB-48M50",null,null,10,11.523047584963946,{"$f":"F841*(1-Elteq!$F$8)","v":11.523047584963946}]
["REIKU-B","PAWVB-48P48",null,null,10,11.277876359751948,{"$f":"F842*(1-Elteq!$F$8)","v":11.277876359751948}]
["REIKU-B","PEDST-10F",null,null,50,0.20645997912589376,{"$f":"F843*(1-Elteq!$F$8)","v":0.20645997912589376}]
["REIKU-B","PEDST-12F",null,null,50,0.20645997912589376,{"$f":"F844*(1-Elteq!$F$8)","v":0.20645997912589376}]
["REIKU-B","PEDST-17F",null,null,50,0.21936372782126209,{"$f":"F845*(1-Elteq!$F$8)","v":0.21936372782126209}]
["REIKU-B","PEDST-17G",null,null,50,0.21936372782126209,{"$f":"F846*(1-Elteq!$F$8)","v":0.21936372782126209}]
["REIKU-B","PEDST-23F",null,null,50,0.41291995825178751,{"$f":"F847*(1-Elteq!$F$8)","v":0.41291995825178751}]
["REIKU-B","PEDST-23G",null,null,50,0.41291995825178751,{"$f":"F848*(1-Elteq!$F$8)","v":0.41291995825178751}]
["REIKU-B","PEDST-29F",null,null,30,0.51614994781473456,{"$f":"F849*(1-Elteq!$F$8)","v":0.51614994781473456}]
["REIKU-B","PEDST-29G",null,null,30,0.51614994781473456,{"$f":"F850*(1-Elteq!$F$8)","v":0.51614994781473456}]
["REIKU-B","PEDST-36G/F",null,null,20,0.80003241911283829,{"$f":"F851*(1-Elteq!$F$8)","v":0.80003241911283829}]
["REIKU-B","PEDST-48G/F",null,null,10,0.98068490084799531,{"$f":"F852*(1-Elteq!$F$8)","v":0.98068490084799531}]
["REIKU-B","PKNOB-07M081",null,null,50,2.2581560216894632,{"$f":"F853*(1-Elteq!$F$8)","v":2.2581560216894632}]
["REIKU-B","PKNOB-07M121",null,null,50,2.2581560216894632,{"$f":"F854*(1-Elteq!$F$8)","v":2.2581560216894632}]
["REIKU-B","PMAOB-07P07",null,null,30,3.4840121477494579,{"$f":"F855*(1-Elteq!$F$8)","v":3.4840121477494579}]
["REIKU-B","PMAOB-10P09",null,null,30,3.4840121477494579,{"$f":"F856*(1-Elteq!$F$8)","v":3.4840121477494579}]
["REIKU-B","PMAOB-12P11",null,null,30,3.8582208599151402,{"$f":"F857*(1-Elteq!$F$8)","v":3.8582208599151402}]
["REIKU-B","PMAOB-17P16",null,null,30,4.3356595616437694,{"$f":"F858*(1-Elteq!$F$8)","v":4.3356595616437694}]
["REIKU-B","PMAOB-23P21",null,null,30,6.684141824200811,{"$f":"F859*(1-Elteq!$F$8)","v":6.684141824200811}]
["REIKU-B","PMAOB-29P29",null,null,20,8.2454954163403791,{"$f":"F860*(1-Elteq!$F$8)","v":8.2454954163403791}]
["REIKU-B","PMAVB-07P07",null,null,30,3.8195096138290343,{"$f":"F861*(1-Elteq!$F$8)","v":3.8195096138290343}]
["REIKU-B","PMAVB-10P09",null,null,30,3.8324133625244037,{"$f":"F862*(1-Elteq!$F$8)","v":3.8324133625244037}]
["REIKU-B","PMAVB-12P11",null,null,30,4.2453333207761919,{"$f":"F863*(1-Elteq!$F$8)","v":4.2453333207761919}]
["REIKU-B","PMAVB-17P16",null,null,30,4.7614832685909265,{"$f":"F864*(1-Elteq!$F$8)","v":4.7614832685909265}]
["REIKU-B","PMAVB-23P21",null,null,30,7.3293292589692287,{"$f":"F865*(1-Elteq!$F$8)","v":7.3293292589692287}]
["REIKU-B","PMAVB-29P29",null,null,20,9.084239081539323,{"$f":"F866*(1-Elteq!$F$8)","v":9.084239081539323}]
["REIKU-B","PMGMB-M20",null,null,50,1.1791104704088486,{"$f":"F867*(1-Elteq!$F$8)","v":1.1791104704088486}]
["REIKU-B","PMGMB-M25",null,null,50,1.2774711208414677,{"$f":"F868*(1-Elteq!$F$8)","v":1.2774711208414677}]
["REIKU-B","PMGMB-M32",null,null,25,3.1090730347142252,{"$f":"F869*(1-Elteq!$F$8)","v":3.1090730347142252}]
["REIKU-B","PMGMB-M40",null,null,25,3.2724393625367196,{"$f":"F870*(1-Elteq!$F$8)","v":3.2724393625367196}]
["REIKU-B","PMGOB-07M12Z",null,null,30,6.0389543894323916,{"$f":"F871*(1-Elteq!$F$8)","v":6.0389543894323916}]
["REIKU-B","PMGOB-07P07",null,null,50,2.6323647338551464,{"$f":"F872*(1-Elteq!$F$8)","v":2.6323647338551464}]
["REIKU-B","PMGOB-07P07Z",null,null,30,6.0389543894323916,{"$f":"F873*(1-Elteq!$F$8)","v":6.0389543894323916}]
["REIKU-B","PMGOB-10M16",null,null,30,2.6323647338551464,{"$f":"F874*(1-Elteq!$F$8)","v":2.6323647338551464}]
["REIKU-B","PMGOB-10M16Z",null,null,30,6.0389543894323916,{"$f":"F875*(1-Elteq!$F$8)","v":6.0389543894323916}]
["REIKU-B","PMGOB-10M20",null,null,30,2.6323647338551464,{"$f":"F876*(1-Elteq!$F$8)","v":2.6323647338551464}]
["REIKU-B","PMGOB-10P09",null,null,30,2.6323647338551464,{"$f":"F877*(1-Elteq!$F$8)","v":2.6323647338551464}]
["REIKU-B","PMGOB-10P09Z",null,null,30,6.0389543894323916,{"$f":"F878*(1-Elteq!$F$8)","v":6.0389543894323916}]
["REIKU-B","PMGOB-12M16",null,null,30,3.1227071842791427,{"$f":"F879*(1-Elteq!$F$8)","v":3.1227071842791427}]
["REIKU-B","PMGOB-12M16Z",null,null,30,6.6196230807239651,{"$f":"F880*(1-Elteq!$F$8)","v":6.6196230807239651}]
["REIKU-B","PMGOB-12M20",null,null,30,3.1227071842791427,{"$f":"F881*(1-Elteq!$F$8)","v":3.1227071842791427}]
["REIKU-B","PMGOB-12M20Z",null,null,30,7.4454629972275459,{"$f":"F882*(1-Elteq!$F$8)","v":7.4454629972275459}]
["REIKU-B","PMGOB-12P11",null,null,30,3.1227071842791427,{"$f":"F883*(1-Elteq!$F$8)","v":3.1227071842791427}]
["REIKU-B","PMGOB-12P11Z",null,null,30,6.6196230807239651,{"$f":"F884*(1-Elteq!$F$8)","v":6.6196230807239651}]
["REIKU-B","PMGOB-12P13Z",null,null,30,7.4454629972275459,{"$f":"F885*(1-Elteq!$F$8)","v":7.4454629972275459}]
["REIKU-B","PMGOB-17M20",null,null,30,3.7937021164382991,{"$f":"F886*(1-Elteq!$F$8)","v":3.7937021164382991}]
["REIKU-B","PMGOB-17M20Z",null,null,30,14.245738559686664,{"$f":"F887*(1-Elteq!$F$8)","v":14.245738559686664}]
["REIKU-B","PMGOB-17M25",null,null,30,3.7937021164382991,{"$f":"F888*(1-Elteq!$F$8)","v":3.7937021164382991}]
["REIKU-B","PMGOB-17P13",null,null,30,3.7549908703521941,{"$f":"F889*(1-Elteq!$F$8)","v":3.7549908703521941}]
["REIKU-B","PMGOB-17P16",null,null,30,3.7937021164382991,{"$f":"F890*(1-Elteq!$F$8)","v":3.7937021164382991}]
["REIKU-B","PMGOB-17P16Z",null,null,30,14.245738559686664,{"$f":"F891*(1-Elteq!$F$8)","v":14.245738559686664}]
["REIKU-B","PMGOB-23M25",null,null,30,6.5163930911610208,{"$f":"F892*(1-Elteq!$F$8)","v":6.5163930911610208}]
["REIKU-B","PMGOB-23M25Z",null,null,30,17.058755775276968,{"$f":"F893*(1-Elteq!$F$8)","v":17.058755775276968}]
["REIKU-B","PMGOB-23M32",null,null,30,6.5163930911610208,{"$f":"F894*(1-Elteq!$F$8)","v":6.5163930911610208}]
["REIKU-B","PMGOB-23P21",null,null,30,6.5163930911610208,{"$f":"F895*(1-Elteq!$F$8)","v":6.5163930911610208}]
["REIKU-B","PMGOB-23P21Z",null,null,30,17.058755775276968,{"$f":"F896*(1-Elteq!$F$8)","v":17.058755775276968}]
["REIKU-B","PMGOB-29M32",null,null,20,7.8454792067839625,{"$f":"F897*(1-Elteq!$F$8)","v":7.8454792067839625}]
["REIKU-B","PMGOB-29M32Z",null,null,20,22.310581494291895,{"$f":"F898*(1-Elteq!$F$8)","v":22.310581494291895}]
["REIKU-B","PMGOB-29M40",null,null,20,7.8454792067839625,{"$f":"F899*(1-Elteq!$F$8)","v":7.8454792067839625}]
["REIKU-B","PMGOB-29P29",null,null,20,7.8454792067839625,{"$f":"F900*(1-Elteq!$F$8)","v":7.8454792067839625}]
["REIKU-B","PMGOB-29P29Z",null,null,20,22.310581494291895,{"$f":"F901*(1-Elteq!$F$8)","v":22.310581494291895}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"PMGOB-36M40Z",null,null,10,29.678621999347232,{"$f":"F902*(1-Elteq!$F$8)","v":29.678621999347232}]
["REIKU-B","PMGOB-36M50",null,null,10,12.542443731898043,{"$f":"F903*(1-Elteq!$F$8)","v":12.542443731898043}]
["REIKU-B","PMGOB-36P36",null,null,10,12.542443731898043,{"$f":"F904*(1-Elteq!$F$8)","v":12.542443731898043}]
["REIKU-B","PMGOB-36P36Z",null,null,10,29.678621999347232,{"$f":"F905*(1-Elteq!$F$8)","v":29.678621999347232}]
["REIKU-B","PMGOB-48M63",null,null,10,15.265134706620771,{"$f":"F906*(1-Elteq!$F$8)","v":15.265134706620771}]
["REIKU-B","PMGOB-48M63Z",null,null,10,43.627574339040414,{"$f":"F907*(1-Elteq!$F$8)","v":43.627574339040414}]
["REIKU-B","PMGOB-48P48",null,null,10,15.265134706620771,{"$f":"F908*(1-Elteq!$F$8)","v":15.265134706620771}]
["REIKU-B","PMGOB-48P48Z",null,null,10,43.627574339040414,{"$f":"F909*(1-Elteq!$F$8)","v":43.627574339040414}]
["REIKU-B","PMGVB-07M12Z",null,null,30,6.3873556042073378,{"$f":"F910*(1-Elteq!$F$8)","v":6.3873556042073378}]
["REIKU-B","PMGVB-07P07",null,null,50,2.9807659486300917,{"$f":"F911*(1-Elteq!$F$8)","v":2.9807659486300917}]
["REIKU-B","PMGVB-07P07Z",null,null,30,6.3873556042073378,{"$f":"F912*(1-Elteq!$F$8)","v":6.3873556042073378}]
["REIKU-B","PMGVB-10M16",null,null,30,3.0065734460208282,{"$f":"F913*(1-Elteq!$F$8)","v":3.0065734460208282}]
["REIKU-B","PMGVB-10M16Z",null,null,30,6.4131631015980748,{"$f":"F914*(1-Elteq!$F$8)","v":6.4131631015980748}]
["REIKU-B","PMGVB-10M20",null,null,30,3.0452846921069332,{"$f":"F915*(1-Elteq!$F$8)","v":3.0452846921069332}]
["REIKU-B","PMGVB-10P09",null,null,30,3.0065734460208282,{"$f":"F916*(1-Elteq!$F$8)","v":3.0065734460208282}]
["REIKU-B","PMGVB-10P09Z",null,null,30,6.4002593529027063,{"$f":"F917*(1-Elteq!$F$8)","v":6.4002593529027063}]
["REIKU-B","PMGVB-12M16",null,null,30,3.5098196451401935,{"$f":"F918*(1-Elteq!$F$8)","v":3.5098196451401935}]
["REIKU-B","PMGVB-12M16Z",null,null,30,6.9938317928896518,{"$f":"F919*(1-Elteq!$F$8)","v":6.9938317928896518}]
["REIKU-B","PMGVB-12M20",null,null,30,3.5485308912262981,{"$f":"F920*(1-Elteq!$F$8)","v":3.5485308912262981}]
["REIKU-B","PMGVB-12M20Z",null,null,30,7.8712867041746994,{"$f":"F921*(1-Elteq!$F$8)","v":7.8712867041746994}]
["REIKU-B","PMGVB-12P11",null,null,30,3.5227233938355633,{"$f":"F922*(1-Elteq!$F$8)","v":3.5227233938355633}]
["REIKU-B","PMGVB-12P11Z",null,null,30,6.9938317928896518,{"$f":"F923*(1-Elteq!$F$8)","v":6.9938317928896518}]
["REIKU-B","PMGVB-12P13Z",null,null,30,7.8454792067839625,{"$f":"F924*(1-Elteq!$F$8)","v":7.8454792067839625}]
["REIKU-B","PMGVB-17M20",null,null,30,4.2324295720808225,{"$f":"F925*(1-Elteq!$F$8)","v":4.2324295720808225}]
["REIKU-B","PMGVB-17M20Z",null,null,30,14.684466015329193,{"$f":"F926*(1-Elteq!$F$8)","v":14.684466015329193}]
["REIKU-B","PMGVB-17M25",null,null,30,4.2582370694715594,{"$f":"F927*(1-Elteq!$F$8)","v":4.2582370694715594}]
["REIKU-B","PMGVB-17P13",null,null,30,4.1808145772993504,{"$f":"F928*(1-Elteq!$F$8)","v":4.1808145772993504}]
["REIKU-B","PMGVB-17P16",null,null,30,4.2324295720808225,{"$f":"F929*(1-Elteq!$F$8)","v":4.2324295720808225}]
["REIKU-B","PMGVB-17P16Z",null,null,30,14.671562266633828,{"$f":"F930*(1-Elteq!$F$8)","v":14.671562266633828}]
["REIKU-B","PMGVB-23M25",null,null,30,7.1744842746248088,{"$f":"F931*(1-Elteq!$F$8)","v":7.1744842746248088}]
["REIKU-B","PMGVB-23M25Z",null,null,30,17.703943210045388,{"$f":"F932*(1-Elteq!$F$8)","v":17.703943210045388}]
["REIKU-B","PMGVB-23M32",null,null,30,7.2648105154923881,{"$f":"F933*(1-Elteq!$F$8)","v":7.2648105154923881}]
["REIKU-B","PMGVB-23P21",null,null,30,7.2002917720155457,{"$f":"F934*(1-Elteq!$F$8)","v":7.2002917720155457}]
["REIKU-B","PMGVB-23P21Z",null,null,30,17.703943210045388,{"$f":"F935*(1-Elteq!$F$8)","v":17.703943210045388}]
["REIKU-B","PMGVB-29M32",null,null,20,8.6842228719829055,{"$f":"F936*(1-Elteq!$F$8)","v":8.6842228719829055}]
["REIKU-B","PMGVB-29M32Z",null,null,20,23.162228908186215,{"$f":"F937*(1-Elteq!$F$8)","v":23.162228908186215}]
["REIKU-B","PMGVB-29M40",null,null,20,8.8648753537180642,{"$f":"F938*(1-Elteq!$F$8)","v":8.8648753537180642}]
["REIKU-B","PMGVB-29P29",null,null,20,8.6971266206782758,{"$f":"F939*(1-Elteq!$F$8)","v":8.6971266206782758}]
["REIKU-B","PMGVB-29P29Z",null,null,20,23.162228908186215,{"$f":"F940*(1-Elteq!$F$8)","v":23.162228908186215}]
["REIKU-B","PMGVB-36M40Z",null,null,10,30.981900617579424,{"$f":"F941*(1-Elteq!$F$8)","v":30.981900617579424}]
["REIKU-B","PMGVB-36M50",null,null,10,14.052182329256139,{"$f":"F942*(1-Elteq!$F$8)","v":14.052182329256139}]
["REIKU-B","PMGVB-36P36",null,null,10,13.729588611871932,{"$f":"F943*(1-Elteq!$F$8)","v":13.729588611871932}]
["REIKU-B","PMGVB-36P36Z",null,null,10,30.865766879321122,{"$f":"F944*(1-Elteq!$F$8)","v":30.865766879321122}]
["REIKU-B","PMGVB-48M63",null,null,10,17.17488951353528,{"$f":"F945*(1-Elteq!$F$8)","v":17.17488951353528}]
["REIKU-B","PMGVB-48M63Z",null,null,10,45.550232894650328,{"$f":"F946*(1-Elteq!$F$8)","v":45.550232894650328}]
["REIKU-B","PMGVB-48P48",null,null,10,16.723258309197401,{"$f":"F947*(1-Elteq!$F$8)","v":16.723258309197401}]
["REIKU-B","PMGVB-48P48Z",null,null,10,45.085697941617042,{"$f":"F948*(1-Elteq!$F$8)","v":45.085697941617042}]
["REIKU-B","PMSOB-07P07",null,null,30,3.6646646294846144,{"$f":"F949*(1-Elteq!$F$8)","v":3.6646646294846144}]
["REIKU-B","PMSVB-07P07",null,null,30,4.0130658442595601,{"$f":"F950*(1-Elteq!$F$8)","v":4.0130658442595601}]
["REIKU-B","PMWOB-10P09",null,null,30,3.6646646294846144,{"$f":"F951*(1-Elteq!$F$8)","v":3.6646646294846144}]
["REIKU-B","PMWOB-12M16",null,null,30,3.7162796242660856,{"$f":"F952*(1-Elteq!$F$8)","v":3.7162796242660856}]
["REIKU-B","PMWOB-12P11",null,null,30,3.7162796242660856,{"$f":"F953*(1-Elteq!$F$8)","v":3.7162796242660856}]
["REIKU-B","PMWOB-17M20",null,null,30,4.1679108286039801,{"$f":"F954*(1-Elteq!$F$8)","v":4.1679108286039801}]
["REIKU-B","PMWOB-17P13",null,null,30,4.090488336431771,{"$f":"F955*(1-Elteq!$F$8)","v":4.090488336431771}]
["REIKU-B","PMWOB-17P16",null,null,30,4.1679108286039801,{"$f":"F956*(1-Elteq!$F$8)","v":4.1679108286039801}]
["REIKU-B","PMWOB-23M25",null,null,30,6.4131631015980748,{"$f":"F957*(1-Elteq!$F$8)","v":6.4131631015980748}]
["REIKU-B","PMWOB-23P21",null,null,30,7.1873880233201763,{"$f":"F958*(1-Elteq!$F$8)","v":7.1873880233201763}]
["REIKU-B","PMWOB-29M32",null,null,20,7.9099979502608058,{"$f":"F959*(1-Elteq!$F$8)","v":7.9099979502608058}]
["REIKU-B","PMWOB-29P29",null,null,20,7.9099979502608058,{"$f":"F960*(1-Elteq!$F$8)","v":7.9099979502608058}]
["REIKU-B","PMWOB-36M40",null,null,10,13.277957407534041,{"$f":"F961*(1-Elteq!$F$8)","v":13.277957407534041}]
["REIKU-B","PMWOB-36P36",null,null,10,13.277957407534041,{"$f":"F962*(1-Elteq!$F$8)","v":13.277957407534041}]
["REIKU-B","PMWOB-48M50",null,null,10,19.807254247390436,{"$f":"F963*(1-Elteq!$F$8)","v":19.807254247390436}]
["REIKU-B","PMWOB-48P48",null,null,10,19.807254247390436,{"$f":"F964*(1-Elteq!$F$8)","v":19.807254247390436}]
["REIKU-B","PMWVB-10P09",null,null,30,4.0259695929549286,{"$f":"F965*(1-Elteq!$F$8)","v":4.0259695929549286}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"PMWVB-12M16",null,null,30,4.1033920851271395,{"$f":"F966*(1-Elteq!$F$8)","v":4.1033920851271395}]
["REIKU-B","PMWVB-12P11",null,null,30,4.1033920851271395,{"$f":"F967*(1-Elteq!$F$8)","v":4.1033920851271395}]
["REIKU-B","PMWVB-17M20",null,null,30,4.6066382842465039,{"$f":"F968*(1-Elteq!$F$8)","v":4.6066382842465039}]
["REIKU-B","PMWVB-17P13",null,null,30,4.5034082946835579,{"$f":"F969*(1-Elteq!$F$8)","v":4.5034082946835579}]
["REIKU-B","PMWVB-17P16",null,null,30,4.5937345355511363,{"$f":"F970*(1-Elteq!$F$8)","v":4.5937345355511363}]
["REIKU-B","PMWVB-23M25",null,null,30,7.058350536366496,{"$f":"F971*(1-Elteq!$F$8)","v":7.058350536366496}]
["REIKU-B","PMWVB-23P21",null,null,30,7.8325754580885949,{"$f":"F972*(1-Elteq!$F$8)","v":7.8325754580885949}]
["REIKU-B","PMWVB-29M32",null,null,20,8.7616453641551164,{"$f":"F973*(1-Elteq!$F$8)","v":8.7616453641551164}]
["REIKU-B","PMWVB-29P29",null,null,20,8.7616453641551164,{"$f":"F974*(1-Elteq!$F$8)","v":8.7616453641551164}]
["REIKU-B","PMWVB-36M40",null,null,10,14.581236025766247,{"$f":"F975*(1-Elteq!$F$8)","v":14.581236025766247}]
["REIKU-B","PMWVB-36P36",null,null,10,14.465102287507936,{"$f":"F976*(1-Elteq!$F$8)","v":14.465102287507936}]
["REIKU-B","PMWVB-48M50",null,null,10,21.510549075179064,{"$f":"F977*(1-Elteq!$F$8)","v":21.510549075179064}]
["REIKU-B","PMWVB-48P48",null,null,10,21.265377849967059,{"$f":"F978*(1-Elteq!$F$8)","v":21.265377849967059}]
["REIKU-B","POFHB-23/29",null,null,25,5.4929207018028405,{"$f":"F979*(1-Elteq!$F$8)","v":5.4929207018028405}]
["REIKU-B","POFHB-36",null,null,10,6.6410311763599923,{"$f":"F980*(1-Elteq!$F$8)","v":6.6410311763599923}]
["REIKU-B","POFHB-36/36",null,null,10,6.6410311763599923,{"$f":"F981*(1-Elteq!$F$8)","v":6.6410311763599923}]
["REIKU-B","POGTB-70",null,null,10,19.825166459191276,{"$f":"F982*(1-Elteq!$F$8)","v":19.825166459191276}]
["REIKU-B","POKGB-70",null,null,10,9.680597377824828,{"$f":"F983*(1-Elteq!$F$8)","v":9.680597377824828}]
["REIKU-B","POSSB-90K",null,null,10,28.984161490045732,{"$f":"F984*(1-Elteq!$F$8)","v":28.984161490045732}]
["REIKU-B","POSSB-90M",null,null,10,49.389011179037922,{"$f":"F985*(1-Elteq!$F$8)","v":49.389011179037922}]
["REIKU-B","PPREB-12F",null,null,50,0.60673554531467833,{"$f":"F986*(1-Elteq!$F$8)","v":0.60673554531467833}]
["REIKU-B","PPREB-17F",null,null,50,0.65484240893995216,{"$f":"F987*(1-Elteq!$F$8)","v":0.65484240893995216}]
["REIKU-B","PPREB-23'F",null,null,50,0.66760545439155561,{"$f":"F988*(1-Elteq!$F$8)","v":0.66760545439155561}]
["REIKU-B","PPREB-29F",null,null,50,1.2081695179033061,{"$f":"F989*(1-Elteq!$F$8)","v":1.2081695179033061}]
["REIKU-B","PPREB-36F",null,null,30,1.3428687360540725,{"$f":"F990*(1-Elteq!$F$8)","v":1.3428687360540725}]
["REIKU-B","PPREB-48F",null,null,30,1.4763898269323841,{"$f":"F991*(1-Elteq!$F$8)","v":1.4763898269323841}]
["REIKU-B","PPRTB-10",null,null,50,1.7754723579907112,{"$f":"F992*(1-Elteq!$F$8)","v":1.7754723579907112}]
["REIKU-B","PPRTB-12",null,null,50,2.1609367515018527,{"$f":"F993*(1-Elteq!$F$8)","v":2.1609367515018527}]
["REIKU-B","PPRTB-14",null,null,50,2.277744143474925,{"$f":"F994*(1-Elteq!$F$8)","v":2.277744143474925}]
["REIKU-B","PPRTB-17",null,null,50,2.4062322746453062,{"$f":"F995*(1-Elteq!$F$8)","v":2.4062322746453062}]
["REIKU-B","PPRTB-24",null,null,25,3.3290106712325831,{"$f":"F996*(1-Elteq!$F$8)","v":3.3290106712325831}]
["REIKU-B","PPRTB-29",null,null,25,3.7845594999275676,{"$f":"F997*(1-Elteq!$F$8)","v":3.7845594999275676}]
["REIKU-B","PPRTB-34",null,null,25,4.8708682452771468,{"$f":"F998*(1-Elteq!$F$8)","v":4.8708682452771468}]
["REIKU-B","PPRTB-45",null,null,25,6.0506229042051851,{"$f":"F999*(1-Elteq!$F$8)","v":6.0506229042051851}]
["REIKU-B","PPRTB-68",null,null,10,18.683134995693091,{"$f":"F1000*(1-Elteq!$F$8)","v":18.683134995693091}]
["REIKU-B","PSNOB-07M081",null,null,50,4.6324457816372417,{"$f":"F1001*(1-Elteq!$F$8)","v":4.6324457816372417}]
["REIKU-B","PSNOB-07M121",null,null,50,4.6324457816372417,{"$f":"F1002*(1-Elteq!$F$8)","v":4.6324457816372417}]
["REIKU-B","PURMB-70G",null,null,"10/30",27.175469084644494,{"$f":"F1003*(1-Elteq!$F$8)","v":27.175469084644494}]
["REIKU-B","PURRB-07G",null,null,100,2.0145976358992237,{"$f":"F1004*(1-Elteq!$F$8)","v":2.0145976358992237}]
["REIKU-B","PURRB-10F",null,null,100,2.0617227267974512,{"$f":"F1005*(1-Elteq!$F$8)","v":2.0617227267974512}]
["REIKU-B","PURRB-12F",null,null,50,2.6115154539434378,{"$f":"F1006*(1-Elteq!$F$8)","v":2.6115154539434378}]
["REIKU-B","PURRB-17F",null,null,50,3.4362045446624183,{"$f":"F1007*(1-Elteq!$F$8)","v":3.4362045446624183}]
["REIKU-B","PURRB-17G",null,null,50,3.4362045446624183,{"$f":"F1008*(1-Elteq!$F$8)","v":3.4362045446624183}]
["REIKU-B","PURRB-23F",null,null,50,4.7517799989046008,{"$f":"F1009*(1-Elteq!$F$8)","v":4.7517799989046008}]
["REIKU-B","PURRB-23G",null,null,50,4.7517799989046008,{"$f":"F1010*(1-Elteq!$F$8)","v":4.7517799989046008}]
["REIKU-B","PURRB-29F",null,null,30,6.2833454530969934,{"$f":"F1011*(1-Elteq!$F$8)","v":6.2833454530969934}]
["REIKU-B","PURRB-29G",null,null,30,6.2833454530969934,{"$f":"F1012*(1-Elteq!$F$8)","v":6.2833454530969934}]
["REIKU-B","PURRB-36F",null,null,30,8.4628809071400131,{"$f":"F1013*(1-Elteq!$F$8)","v":8.4628809071400131}]
["REIKU-B","PURRB-36G",null,null,30,8.4628809071400131,{"$f":"F1014*(1-Elteq!$F$8)","v":8.4628809071400131}]
["REIKU-B","PURRB-42M",null,null,30,10.838770906592311,{"$f":"F1015*(1-Elteq!$F$8)","v":10.838770906592311}]
["REIKU-B","PURRB-48F",null,null,30,10.976219088378809,{"$f":"F1016*(1-Elteq!$F$8)","v":10.976219088378809}]
["REIKU-B","PURRB-48G",null,null,30,10.976219088378809,{"$f":"F1017*(1-Elteq!$F$8)","v":10.976219088378809}]
["REIKU-B","PURRB-52G",null,null,"10/30",15.904718178151761,{"$f":"F1018*(1-Elteq!$F$8)","v":15.904718178151761}]
["REIKU-B","PURRB-68G",null,null,30,23.503639085490946,{"$f":"F1019*(1-Elteq!$F$8)","v":23.503639085490946}]
["REIKU-B","PURRB-70G",null,null,"10/30",22.423689085739891,{"$f":"F1020*(1-Elteq!$F$8)","v":22.423689085739891}]
["REIKU-B","PURRB-95G",null,null,"10/30",38.44621999113722,{"$f":"F1021*(1-Elteq!$F$8)","v":38.44621999113722}]
["REIKU-B","PURVB-36G",null,null,30,11.242083142862974,{"$f":"F1022*(1-Elteq!$F$8)","v":11.242083142862974}]
["REIKU-B","PURVB-48F",null,null,"10/30",14.351553723964351,{"$f":"F1023*(1-Elteq!$F$8)","v":14.351553723964351}]
["REIKU-B","PURVB-52G",null,null,"10/30",18.025347268571998,{"$f":"F1024*(1-Elteq!$F$8)","v":18.025347268571998}]
["REIKU-B","PURVB-70G",null,null,"10/30",27.901980902658842,{"$f":"F1025*(1-Elteq!$F$8)","v":27.901980902658842}]
["REIKU-B","PWNOB-07M081",null,null,50,4.6324457816372417,{"$f":"F1026*(1-Elteq!$F$8)","v":4.6324457816372417}]
["REIKU-B","PWNOB-07M121",null,null,50,4.6324457816372417,{"$f":"F1027*(1-Elteq!$F$8)","v":4.6324457816372417}]
["REIKU-B","PWNOB-07M181",null,null,50,4.6324457816372417,{"$f":"F1028*(1-Elteq!$F$8)","v":4.6324457816372417}]
["REIKU-B","PWNOB-07M301",null,null,50,4.8647132581538735,{"$f":"F1029*(1-Elteq!$F$8)","v":4.8647132581538735}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"TKBSB- 7,5",null,null,10,0.68724090893248357,{"$f":"F1030*(1-Elteq!$F$8)","v":0.68724090893248357}]
["REIKU-B","TKBSB-10",null,null,10,0.68724090893248357,{"$f":"F1031*(1-Elteq!$F$8)","v":0.68724090893248357}]
["REIKU-B","TKBSB-12,5",null,null,10,0.68724090893248357,{"$f":"F1032*(1-Elteq!$F$8)","v":0.68724090893248357}]
["REIKU-B","TKBSB-14",null,null,10,0.68724090893248357,{"$f":"F1033*(1-Elteq!$F$8)","v":0.68724090893248357}]
["REIKU-B","TKBSB-15,5",null,null,10,0.68724090893248357,{"$f":"F1034*(1-Elteq!$F$8)","v":0.68724090893248357}]
["REIKU-B","TKBSB-19,5",null,null,10,0.68724090893248357,{"$f":"F1035*(1-Elteq!$F$8)","v":0.68724090893248357}]
["REIKU-B","TKBSB-22",null,null,10,0.98177272704640517,{"$f":"F1036*(1-Elteq!$F$8)","v":0.98177272704640517}]
["REIKU-B","TKBSB-28",null,null,10,0.98177272704640517,{"$f":"F1037*(1-Elteq!$F$8)","v":0.98177272704640517}]
["REIKU-B","TKKSB23BLIND",null,null,10,6.0935400637868558,{"$f":"F1038*(1-Elteq!$F$8)","v":6.0935400637868558}]
["REIKU-B","TKKSB29BLIND",null,null,10,6.3335176649393894,{"$f":"F1039*(1-Elteq!$F$8)","v":6.3335176649393894}]
["REIKU-B","TKKSB42BLIND",null,null,10,9.4479916614583743,{"$f":"F1040*(1-Elteq!$F$8)","v":9.4479916614583743}]
["REIKU-B","TKKSB48BLIND",null,null,10,10.858406361133243,{"$f":"F1041*(1-Elteq!$F$8)","v":10.858406361133243}]
["REIKU-B","TKKSB36BLIND",null,null,10,8.5456901737250881,{"$f":"F1042*(1-Elteq!$F$8)","v":8.5456901737250881}]
["REIKU-B","TKKSB52BLIND",null,null,10,12.323080004076779,{"$f":"F1043*(1-Elteq!$F$8)","v":12.323080004076779}]
["REIKU-B","TKKSB70BLIND",null,null,10,12.105493349936667,{"$f":"F1044*(1-Elteq!$F$8)","v":12.105493349936667}]
["REIKU-B","TKKSB-36B01",null,null,10,7.3770487824464395,{"$f":"F1045*(1-Elteq!$F$8)","v":7.3770487824464395}]
["REIKU-B","TKKSB-48B01",null,null,10,9.5624663614319871,{"$f":"F1046*(1-Elteq!$F$8)","v":9.5624663614319871}]
["REIKU-B","TKKSB-52B01",null,null,10,10.774630160632581,{"$f":"F1047*(1-Elteq!$F$8)","v":10.774630160632581}]
["REIKU-B","TKKSB-52B02",null,null,10,10.774630160632581,{"$f":"F1048*(1-Elteq!$F$8)","v":10.774630160632581}]
["REIKU-B","TKKSB-70B01",null,null,10,10.774630160632581,{"$f":"F1049*(1-Elteq!$F$8)","v":10.774630160632581}]
["REIKU-B","TKKSB-70B02",null,null,10,10.774630160632581,{"$f":"F1050*(1-Elteq!$F$8)","v":10.774630160632581}]
["REIKU-B","TKKSB-70B03",null,null,10,10.774630160632581,{"$f":"F1051*(1-Elteq!$F$8)","v":10.774630160632581}]
["REIKU-B","TKKSB-70B04",null,null,10,10.774630160632581,{"$f":"F1052*(1-Elteq!$F$8)","v":10.774630160632581}]
["REIKU-B","TKKSB-70B05",null,null,10,10.774630160632581,{"$f":"F1053*(1-Elteq!$F$8)","v":10.774630160632581}]
["REIKU-B","TKKSB-70B06",null,null,10,10.774630160632581,{"$f":"F1054*(1-Elteq!$F$8)","v":10.774630160632581}]
["REIKU-B","TKKSB-70B07",null,null,10,10.774630160632581,{"$f":"F1055*(1-Elteq!$F$8)","v":10.774630160632581}]
["REIKU-B","TKKSB-70B12",null,null,10,10.774679124167523,{"$f":"F1056*(1-Elteq!$F$8)","v":10.774679124167523}]
["REIKU-B","TKKSB-70B13",null,null,10,10.774679124167523,{"$f":"F1057*(1-Elteq!$F$8)","v":10.774679124167523}]
["REIKU-B","TKKSB 70B14",null,null,10,10.774679124167523,{"$f":"F1058*(1-Elteq!$F$8)","v":10.774679124167523}]
["REIKU-B","TPDVW-07",null,null,50,10.774679124167523,{"$f":"F1059*(1-Elteq!$F$8)","v":10.774679124167523}]
["REIKU-B","TPDVW-10",null,null,50,0.19355623043052539,{"$f":"F1060*(1-Elteq!$F$8)","v":0.19355623043052539}]
["REIKU-B","TPDVW-12",null,null,50,0.20645997912589376,{"$f":"F1061*(1-Elteq!$F$8)","v":0.20645997912589376}]
["REIKU-B","TPDVW-17",null,null,50,0.21936372782126209,{"$f":"F1062*(1-Elteq!$F$8)","v":0.21936372782126209}]
["REIKU-B","TPDVW-23",null,null,30,0.41291995825178751,{"$f":"F1063*(1-Elteq!$F$8)","v":0.41291995825178751}]
["REIKU-B","TPDVW-29",null,null,30,0.51614994781473456,{"$f":"F1064*(1-Elteq!$F$8)","v":0.51614994781473456}]
["REIKU-B","TPDVW-36",null,null,20,0.80003241911283829,{"$f":"F1065*(1-Elteq!$F$8)","v":0.80003241911283829}]
["REIKU-B","TPDVW-48",null,null,10,0.98068490084799531,{"$f":"F1066*(1-Elteq!$F$8)","v":0.98068490084799531}]
["REIKU-B","TPRIB-10F",null,null,100,1.4632851020547726,{"$f":"F1067*(1-Elteq!$F$8)","v":1.4632851020547726}]
["REIKU-B","TPRIB-12F",null,null,50,1.6258723356164138,{"$f":"F1068*(1-Elteq!$F$8)","v":1.6258723356164138}]
["REIKU-B","TPRIB-17F",null,null,50,2.7407562228962399,{"$f":"F1069*(1-Elteq!$F$8)","v":2.7407562228962399}]
["REIKU-B","TPRIB-23F",null,null,50,4.1111343343443609,{"$f":"F1070*(1-Elteq!$F$8)","v":4.1111343343443609}]
["REIKU-B","TPRIB-29F",null,null,50,4.9705239974558957,{"$f":"F1071*(1-Elteq!$F$8)","v":4.9705239974558957}]
["REIKU-B","TPRIB-36M",null,null,30,6.2015416229940339,{"$f":"F1072*(1-Elteq!$F$8)","v":6.2015416229940339}]
["REIKU-B","TPRIB-48M",null,null,30,8.6984169955478148,{"$f":"F1073*(1-Elteq!$F$8)","v":8.6984169955478148}]
["REIKU-B","VAKEM",null,null,10,9.4544713614568821,{"$f":"F1074*(1-Elteq!$F$8)","v":9.4544713614568821}]
["REIKU-B","VAKEM-1.5",null,null,10,9.4544713614568821,{"$f":"F1075*(1-Elteq!$F$8)","v":9.4544713614568821}]
["REIKU-B","VMARB-10M16",null,null,30,3.9485471007827186,{"$f":"F1076*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-B","VMARB-10M20",null,null,30,3.9485471007827186,{"$f":"F1077*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-B","VMARB-10P09",null,null,30,3.9485471007827186,{"$f":"F1078*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-B","VMARB-12M16",null,null,30,3.9485471007827186,{"$f":"F1079*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-B","VMARB-12M20",null,null,30,3.9485471007827186,{"$f":"F1080*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-B","VMARB-12P11",null,null,30,3.9485471007827186,{"$f":"F1081*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-B","VMARB-17M20",null,null,30,4.8001945146770293,{"$f":"F1082*(1-Elteq!$F$8)","v":4.8001945146770293}]
["REIKU-B","VMARB-17M25",null,null,30,4.8001945146770293,{"$f":"F1083*(1-Elteq!$F$8)","v":4.8001945146770293}]
["REIKU-B","VMARB-17P13",null,null,30,4.8001945146770293,{"$f":"F1084*(1-Elteq!$F$8)","v":4.8001945146770293}]
["REIKU-B","VMARB-17P16",null,null,30,4.8001945146770293,{"$f":"F1085*(1-Elteq!$F$8)","v":4.8001945146770293}]
["REIKU-B","VMARB-23M32",null,null,30,7.2648105154923881,{"$f":"F1086*(1-Elteq!$F$8)","v":7.2648105154923881}]
["REIKU-B","VMARB-23P21",null,null,30,7.2648105154923881,{"$f":"F1087*(1-Elteq!$F$8)","v":7.2648105154923881}]
["REIKU-B","VMARB-29M32",null,null,30,8.7487416154597462,{"$f":"F1088*(1-Elteq!$F$8)","v":8.7487416154597462}]
["REIKU-B","VMARB-29M40",null,null,20,8.7487416154597462,{"$f":"F1089*(1-Elteq!$F$8)","v":8.7487416154597462}]
["REIKU-B","VMARB-29P29",null,null,20,8.7487416154597462,{"$f":"F1090*(1-Elteq!$F$8)","v":8.7487416154597462}]
["REIKU-B","VMARB-36M40",null,null,10,15.265134706620771,{"$f":"F1091*(1-Elteq!$F$8)","v":15.265134706620771}]
["REIKU-B","VMARB-36M50",null,null,10,15.265134706620771,{"$f":"F1092*(1-Elteq!$F$8)","v":15.265134706620771}]
["REIKU-B","VMARB-36P36",null,null,10,15.265134706620771,{"$f":"F1093*(1-Elteq!$F$8)","v":15.265134706620771}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"VMARB-48M63",null,null,10,20.775035399543064,{"$f":"F1094*(1-Elteq!$F$8)","v":20.775035399543064}]
["REIKU-B","VMARB-48P48",null,null,10,20.775035399543064,{"$f":"F1095*(1-Elteq!$F$8)","v":20.775035399543064}]
["REIKU-B","VMAVB-10M16",null,null,30,4.1291995825178764,{"$f":"F1096*(1-Elteq!$F$8)","v":4.1291995825178764}]
["REIKU-B","VMAVB-10M20",null,null,30,4.1679108286039801,{"$f":"F1097*(1-Elteq!$F$8)","v":4.1679108286039801}]
["REIKU-B","VMAVB-10P09",null,null,30,4.1162958338225071,{"$f":"F1098*(1-Elteq!$F$8)","v":4.1162958338225071}]
["REIKU-B","VMAVB-12M16",null,null,30,4.1162958338225071,{"$f":"F1099*(1-Elteq!$F$8)","v":4.1162958338225071}]
["REIKU-B","VMAVB-12M20",null,null,30,4.1679108286039801,{"$f":"F1100*(1-Elteq!$F$8)","v":4.1679108286039801}]
["REIKU-B","VMAVB-12P11",null,null,30,4.1291995825178764,{"$f":"F1101*(1-Elteq!$F$8)","v":4.1291995825178764}]
["REIKU-B","VMAVB-17M20",null,null,30,5.0066544938029232,{"$f":"F1102*(1-Elteq!$F$8)","v":5.0066544938029232}]
["REIKU-B","VMAVB-17M25",null,null,30,5.0453657398890277,{"$f":"F1103*(1-Elteq!$F$8)","v":5.0453657398890277}]
["REIKU-B","VMAVB-17P13",null,null,30,4.9808469964121862,{"$f":"F1104*(1-Elteq!$F$8)","v":4.9808469964121862}]
["REIKU-B","VMAVB-17P16",null,null,30,4.9937507451075573,{"$f":"F1105*(1-Elteq!$F$8)","v":4.9937507451075573}]
["REIKU-B","VMAVB-23M32",null,null,30,7.5874042328765983,{"$f":"F1106*(1-Elteq!$F$8)","v":7.5874042328765983}]
["REIKU-B","VMAVB-23P21",null,null,30,7.4970779920090189,{"$f":"F1107*(1-Elteq!$F$8)","v":7.4970779920090189}]
["REIKU-B","VMAVB-29M32",null,null,20,9.084239081539323,{"$f":"F1108*(1-Elteq!$F$8)","v":9.084239081539323}]
["REIKU-B","VMAVB-29M32",null,null,20,9.084239081539323,{"$f":"F1109*(1-Elteq!$F$8)","v":9.084239081539323}]
["REIKU-B","VMAVB-29M40",null,null,20,9.2390840658837483,{"$f":"F1110*(1-Elteq!$F$8)","v":9.2390840658837483}]
["REIKU-B","VMAVB-29P29",null,null,20,9.0713353328439563,{"$f":"F1111*(1-Elteq!$F$8)","v":9.0713353328439563}]
["REIKU-B","VMAVB-36M40",null,null,10,15.768380905740136,{"$f":"F1112*(1-Elteq!$F$8)","v":15.768380905740136}]
["REIKU-B","VMAVB-36M50",null,null,10,15.974840884866033,{"$f":"F1113*(1-Elteq!$F$8)","v":15.974840884866033}]
["REIKU-B","VMAVB-36P36",null,null,10,15.66515091617719,{"$f":"F1114*(1-Elteq!$F$8)","v":15.66515091617719}]
["REIKU-B","VMAVB-48M63",null,null,10,21.717009054304945,{"$f":"F1115*(1-Elteq!$F$8)","v":21.717009054304945}]
["REIKU-B","VMAVB-48P48",null,null,10,21.252474101271687,{"$f":"F1116*(1-Elteq!$F$8)","v":21.252474101271687}]
["REIKU-B","VMBRB-10M16",null,null,30,3.9485471007827186,{"$f":"F1117*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-B","VMBRB-10M20",null,null,30,3.9485471007827186,{"$f":"F1118*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-B","VMBRB-10P09",null,null,30,3.9485471007827186,{"$f":"F1119*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-B","VMBRB-10P11",null,null,30,3.9485471007827186,{"$f":"F1120*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-B","VMBRB-10P13",null,null,30,3.9485471007827186,{"$f":"F1121*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-B","VMBRB-12M16",null,null,30,3.9485471007827186,{"$f":"F1122*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-B","VMBRB-12M20",null,null,30,3.9485471007827186,{"$f":"F1123*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-B","VMBRB-12P11",null,null,30,3.9485471007827186,{"$f":"F1124*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-B","VMBRB-12P13",null,null,30,3.9485471007827186,{"$f":"F1125*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-B","VMBRB-17M20",null,null,30,4.8001945146770293,{"$f":"F1126*(1-Elteq!$F$8)","v":4.8001945146770293}]
["REIKU-B","VMBRB-17M25",null,null,30,4.8001945146770293,{"$f":"F1127*(1-Elteq!$F$8)","v":4.8001945146770293}]
["REIKU-B","VMBRB-17P13",null,null,30,4.8001945146770293,{"$f":"F1128*(1-Elteq!$F$8)","v":4.8001945146770293}]
["REIKU-B","VMBRB-17P16",null,null,30,4.8001945146770293,{"$f":"F1129*(1-Elteq!$F$8)","v":4.8001945146770293}]
["REIKU-B","VMBRB-23M32",null,null,30,7.2648105154923881,{"$f":"F1130*(1-Elteq!$F$8)","v":7.2648105154923881}]
["REIKU-B","VMBRB-23P21",null,null,30,7.2648105154923881,{"$f":"F1131*(1-Elteq!$F$8)","v":7.2648105154923881}]
["REIKU-B","VMBRB-29M32",null,null,20,8.7487416154597462,{"$f":"F1132*(1-Elteq!$F$8)","v":8.7487416154597462}]
["REIKU-B","VMBRB-29M40",null,null,20,8.7487416154597462,{"$f":"F1133*(1-Elteq!$F$8)","v":8.7487416154597462}]
["REIKU-B","VMBRB-29P29",null,null,20,8.7487416154597462,{"$f":"F1134*(1-Elteq!$F$8)","v":8.7487416154597462}]
["REIKU-B","VMBRB-36M40",null,null,10,15.265134706620771,{"$f":"F1135*(1-Elteq!$F$8)","v":15.265134706620771}]
["REIKU-B","VMBRB-36M50",null,null,10,15.265134706620771,{"$f":"F1136*(1-Elteq!$F$8)","v":15.265134706620771}]
["REIKU-B","VMBRB-36P36",null,null,10,15.265134706620771,{"$f":"F1137*(1-Elteq!$F$8)","v":15.265134706620771}]
["REIKU-B","VMBRB-48M63",null,null,10,20.775035399543064,{"$f":"F1138*(1-Elteq!$F$8)","v":20.775035399543064}]
["REIKU-B","VMBRB-48P48",null,null,10,20.775035399543064,{"$f":"F1139*(1-Elteq!$F$8)","v":20.775035399543064}]
["REIKU-B","VMBVB-10M16",null,null,30,4.1291995825178764,{"$f":"F1140*(1-Elteq!$F$8)","v":4.1291995825178764}]
["REIKU-B","VMBVB-10M20",null,null,30,4.1679108286039801,{"$f":"F1141*(1-Elteq!$F$8)","v":4.1679108286039801}]
["REIKU-B","VMBVB-10P09",null,null,30,4.1162958338225071,{"$f":"F1142*(1-Elteq!$F$8)","v":4.1162958338225071}]
["REIKU-B","VMBVB-10P11",null,null,30,4.1291995825178764,{"$f":"F1143*(1-Elteq!$F$8)","v":4.1291995825178764}]
["REIKU-B","VMBVB-10P13",null,null,30,4.142103331213244,{"$f":"F1144*(1-Elteq!$F$8)","v":4.142103331213244}]
["REIKU-B","VMBVB-12M16",null,null,30,4.1162958338225071,{"$f":"F1145*(1-Elteq!$F$8)","v":4.1162958338225071}]
["REIKU-B","VMBVB-12M20",null,null,30,4.1679108286039801,{"$f":"F1146*(1-Elteq!$F$8)","v":4.1679108286039801}]
["REIKU-B","VMBVB-12P11",null,null,30,4.1291995825178764,{"$f":"F1147*(1-Elteq!$F$8)","v":4.1291995825178764}]
["REIKU-B","VMBVB-12P13",null,null,30,4.142103331213244,{"$f":"F1148*(1-Elteq!$F$8)","v":4.142103331213244}]
["REIKU-B","VMBVB-17M20",null,null,30,5.0066544938029232,{"$f":"F1149*(1-Elteq!$F$8)","v":5.0066544938029232}]
["REIKU-B","VMBVB-17M25",null,null,30,5.0453657398890277,{"$f":"F1150*(1-Elteq!$F$8)","v":5.0453657398890277}]
["REIKU-B","VMBVB-17P13",null,null,30,4.9808469964121862,{"$f":"F1151*(1-Elteq!$F$8)","v":4.9808469964121862}]
["REIKU-B","VMBVB-17P16",null,null,30,4.9937507451075573,{"$f":"F1152*(1-Elteq!$F$8)","v":4.9937507451075573}]
["REIKU-B","VMBVB-23M32",null,null,30,7.5874042328765983,{"$f":"F1153*(1-Elteq!$F$8)","v":7.5874042328765983}]
["REIKU-B","VMBVB-23P21",null,null,30,7.4970779920090189,{"$f":"F1154*(1-Elteq!$F$8)","v":7.4970779920090189}]
["REIKU-B","VMBVB-29M40",null,null,20,9.2390840658837483,{"$f":"F1155*(1-Elteq!$F$8)","v":9.2390840658837483}]
["REIKU-B","VMBVB-29P29",null,null,20,9.0713353328439563,{"$f":"F1156*(1-Elteq!$F$8)","v":9.0713353328439563}]
["REIKU-B","VMBVB-36M40",null,null,10,15.768380905740136,{"$f":"F1157*(1-Elteq!$F$8)","v":15.768380905740136}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"VMBVB-36M50",null,null,10,15.974840884866033,{"$f":"F1158*(1-Elteq!$F$8)","v":15.974840884866033}]
["REIKU-B","VMBVB-36P36",null,null,10,15.66515091617719,{"$f":"F1159*(1-Elteq!$F$8)","v":15.66515091617719}]
["REIKU-B","VMBVB-48M63",null,null,10,21.717009054304945,{"$f":"F1160*(1-Elteq!$F$8)","v":21.717009054304945}]
["REIKU-B","VMBVB-48P48",null,null,10,21.252474101271687,{"$f":"F1161*(1-Elteq!$F$8)","v":21.252474101271687}]
["REIKU-B","VMEVB-10M16",null,null,30,8.1422654267774366,{"$f":"F1162*(1-Elteq!$F$8)","v":8.1422654267774366}]
["REIKU-B","VMEVB-12M20",null,null,30,9.1874690711022726,{"$f":"F1163*(1-Elteq!$F$8)","v":9.1874690711022726}]
["REIKU-B","VMEVB-17M20",null,null,30,11.923040706342364,{"$f":"F1164*(1-Elteq!$F$8)","v":11.923040706342364}]
["REIKU-B","VMEVB-17M25",null,null,30,11.923063794520367,{"$f":"F1165*(1-Elteq!$F$8)","v":11.923063794520367}]
["REIKU-B","VMEVB-23M32",null,null,30,18.142670665687913,{"$f":"F1166*(1-Elteq!$F$8)","v":18.142670665687913}]
["REIKU-B","VMEVB-29M40",null,null,20,30.220579444552691,{"$f":"F1167*(1-Elteq!$F$8)","v":30.220579444552691}]
["REIKU-B","VMEVB-36M50",null,null,10,53.615075829255552,{"$f":"F1168*(1-Elteq!$F$8)","v":53.615075829255552}]
["REIKU-B","VMEVB-48M50",null,null,10,53.976380792725855,{"$f":"F1169*(1-Elteq!$F$8)","v":53.976380792725855}]
["REIKU-B","VMGRB-10M16",null,null,30,3.0194771947161958,{"$f":"F1170*(1-Elteq!$F$8)","v":3.0194771947161958}]
["REIKU-B","VMGRB-10M20",null,null,30,3.0194771947161958,{"$f":"F1171*(1-Elteq!$F$8)","v":3.0194771947161958}]
["REIKU-B","VMGRB-10P09",null,null,30,3.0194771947161958,{"$f":"F1172*(1-Elteq!$F$8)","v":3.0194771947161958}]
["REIKU-B","VMGRB-12M16",null,null,30,3.5227233938355633,{"$f":"F1173*(1-Elteq!$F$8)","v":3.5227233938355633}]
["REIKU-B","VMGRB-12M20",null,null,30,3.5227233938355633,{"$f":"F1174*(1-Elteq!$F$8)","v":3.5227233938355633}]
["REIKU-B","VMGRB-12P11",null,null,30,3.5227233938355633,{"$f":"F1175*(1-Elteq!$F$8)","v":3.5227233938355633}]
["REIKU-B","VMGRB-17M20",null,null,30,4.2195258233854531,{"$f":"F1176*(1-Elteq!$F$8)","v":4.2195258233854531}]
["REIKU-B","VMGRB-17M25",null,null,30,4.2195258233854531,{"$f":"F1177*(1-Elteq!$F$8)","v":4.2195258233854531}]
["REIKU-B","VMGRB-17P13",null,null,30,4.1808145772993504,{"$f":"F1178*(1-Elteq!$F$8)","v":4.1808145772993504}]
["REIKU-B","VMGRB-17P16",null,null,30,4.2195258233854531,{"$f":"F1179*(1-Elteq!$F$8)","v":4.2195258233854531}]
["REIKU-B","VMGRB-23M25",null,null,30,7.1873880233201763,{"$f":"F1180*(1-Elteq!$F$8)","v":7.1873880233201763}]
["REIKU-B","VMGRB-23M32",null,null,30,7.1873880233201763,{"$f":"F1181*(1-Elteq!$F$8)","v":7.1873880233201763}]
["REIKU-B","VMGRB-23P21",null,null,30,7.1873880233201763,{"$f":"F1182*(1-Elteq!$F$8)","v":7.1873880233201763}]
["REIKU-B","VMGRB-29M32",null,null,20,8.5680891337245928,{"$f":"F1183*(1-Elteq!$F$8)","v":8.5680891337245928}]
["REIKU-B","VMGRB-29M40",null,null,20,8.5680891337245928,{"$f":"F1184*(1-Elteq!$F$8)","v":8.5680891337245928}]
["REIKU-B","VMGRB-29P29",null,null,20,8.5680891337245928,{"$f":"F1185*(1-Elteq!$F$8)","v":8.5680891337245928}]
["REIKU-B","VMGRB-36M40",null,null,10,13.716684863176566,{"$f":"F1186*(1-Elteq!$F$8)","v":13.716684863176566}]
["REIKU-B","VMGRB-36M50",null,null,10,13.716684863176566,{"$f":"F1187*(1-Elteq!$F$8)","v":13.716684863176566}]
["REIKU-B","VMGRB-36P36",null,null,10,13.716684863176566,{"$f":"F1188*(1-Elteq!$F$8)","v":13.716684863176566}]
["REIKU-B","VMGRB-48M63",null,null,10,16.723258309197401,{"$f":"F1189*(1-Elteq!$F$8)","v":16.723258309197401}]
["REIKU-B","VMGRB-48P48",null,null,10,16.723258309197401,{"$f":"F1190*(1-Elteq!$F$8)","v":16.723258309197401}]
["REIKU-B","VMGVB-10M16",null,null,30,3.1872259277559856,{"$f":"F1191*(1-Elteq!$F$8)","v":3.1872259277559856}]
["REIKU-B","VMGVB-10M16Z",null,null,30,6.9551205468035464,{"$f":"F1192*(1-Elteq!$F$8)","v":6.9551205468035464}]
["REIKU-B","VMGVB-10M20",null,null,30,3.2259371738420892,{"$f":"F1193*(1-Elteq!$F$8)","v":3.2259371738420892}]
["REIKU-B","VMGVB-10P09",null,null,30,3.1872259277559856,{"$f":"F1194*(1-Elteq!$F$8)","v":3.1872259277559856}]
["REIKU-B","VMGVB-12M16",null,null,30,3.6904721268753504,{"$f":"F1195*(1-Elteq!$F$8)","v":3.6904721268753504}]
["REIKU-B","VMGVB-12M16Z",null,null,30,8.0519391859098572,{"$f":"F1196*(1-Elteq!$F$8)","v":8.0519391859098572}]
["REIKU-B","VMGVB-12M20",null,null,30,3.7291833729614554,{"$f":"F1197*(1-Elteq!$F$8)","v":3.7291833729614554}]
["REIKU-B","VMGVB-12M20Z",null,null,30,9.0584315841485932,{"$f":"F1198*(1-Elteq!$F$8)","v":9.0584315841485932}]
["REIKU-B","VMGVB-12P11",null,null,30,3.7033758755707202,{"$f":"F1199*(1-Elteq!$F$8)","v":3.7033758755707202}]
["REIKU-B","VMGVB-17M20",null,null,30,4.425985802511347,{"$f":"F1200*(1-Elteq!$F$8)","v":4.425985802511347}]
["REIKU-B","VMGVB-17M20Z",null,null,30,16.387760843117825,{"$f":"F1201*(1-Elteq!$F$8)","v":16.387760843117825}]
["REIKU-B","VMGVB-17M25",null,null,30,4.4517932999020848,{"$f":"F1202*(1-Elteq!$F$8)","v":4.4517932999020848}]
["REIKU-B","VMGVB-17P13",null,null,30,4.3743708077298731,{"$f":"F1203*(1-Elteq!$F$8)","v":4.3743708077298731}]
["REIKU-B","VMGVB-17P16",null,null,30,4.425985802511347,{"$f":"F1204*(1-Elteq!$F$8)","v":4.425985802511347}]
["REIKU-B","VMGVB-23M25",null,null,30,7.4196554998368081,{"$f":"F1205*(1-Elteq!$F$8)","v":7.4196554998368081}]
["REIKU-B","VMGVB-23M25Z",null,null,30,19.626601765655273,{"$f":"F1206*(1-Elteq!$F$8)","v":19.626601765655273}]
["REIKU-B","VMGVB-23M32",null,null,30,7.5099817407043883,{"$f":"F1207*(1-Elteq!$F$8)","v":7.5099817407043883}]
["REIKU-B","VMGVB-23P21",null,null,30,7.4454629972275459,{"$f":"F1208*(1-Elteq!$F$8)","v":7.4454629972275459}]
["REIKU-B","VMGVB-29M32",null,null,20,8.9035865998041697,{"$f":"F1209*(1-Elteq!$F$8)","v":8.9035865998041697}]
["REIKU-B","VMGVB-29M32Z",null,null,20,25.665556155087671,{"$f":"F1210*(1-Elteq!$F$8)","v":25.665556155087671}]
["REIKU-B","VMGVB-29M40",null,null,20,9.0713353328439563,{"$f":"F1211*(1-Elteq!$F$8)","v":9.0713353328439563}]
["REIKU-B","VMGVB-29P29",null,null,20,8.9035865998041697,{"$f":"F1212*(1-Elteq!$F$8)","v":8.9035865998041697}]
["REIKU-B","VMGVB-36M40",null,null,10,14.219931062295936,{"$f":"F1213*(1-Elteq!$F$8)","v":14.219931062295936}]
["REIKU-B","VMGVB-36M40Z",null,null,10,34.1304152992493,{"$f":"F1214*(1-Elteq!$F$8)","v":34.1304152992493}]
["REIKU-B","VMGVB-36M50",null,null,10,14.426391041421827,{"$f":"F1215*(1-Elteq!$F$8)","v":14.426391041421827}]
["REIKU-B","VMGVB-36P36",null,null,10,14.116701072732992,{"$f":"F1216*(1-Elteq!$F$8)","v":14.116701072732992}]
["REIKU-B","VMGVB-48M63",null,null,10,17.652328215263921,{"$f":"F1217*(1-Elteq!$F$8)","v":17.652328215263921}]
["REIKU-B","VMGVB-48M63Z",null,null,10,51.31820856147997,{"$f":"F1218*(1-Elteq!$F$8)","v":51.31820856147997}]
["REIKU-B","VMGVB-48P48",null,null,10,17.213600759621389,{"$f":"F1219*(1-Elteq!$F$8)","v":17.213600759621389}]
["REIKU-B","VMIRB-17M25",null,null,30,11.850585879086339,{"$f":"F1220*(1-Elteq!$F$8)","v":11.850585879086339}]
["REIKU-B","VMIRB-23M25",null,null,30,14.516098833017328,{"$f":"F1221*(1-Elteq!$F$8)","v":14.516098833017328}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"VMIRB-29M40",null,null,20,14.749564387508963,{"$f":"F1222*(1-Elteq!$F$8)","v":14.749564387508963}]
["REIKU-B","VMIRB-36M50",null,null,10,14.962020005641806,{"$f":"F1223*(1-Elteq!$F$8)","v":14.962020005641806}]
["REIKU-B","VMSVB-12/18",null,null,30,7.4841742433136487,{"$f":"F1224*(1-Elteq!$F$8)","v":7.4841742433136487}]
["REIKU-B","VMSVB-17/20",null,null,30,7.5357892380951208,{"$f":"F1225*(1-Elteq!$F$8)","v":7.5357892380951208}]
["REIKU-B","VMSVB-17/22",null,null,30,7.5357892380951208,{"$f":"F1226*(1-Elteq!$F$8)","v":7.5357892380951208}]
["REIKU-B","VMSVB-17/25",null,null,30,7.5357892380951208,{"$f":"F1227*(1-Elteq!$F$8)","v":7.5357892380951208}]
["REIKU-B","VMSVB-23/28",null,null,20,9.0326240867578527,{"$f":"F1228*(1-Elteq!$F$8)","v":9.0326240867578527}]
["REIKU-B","VMSVB-29/32",null,null,20,11.252097224678849,{"$f":"F1229*(1-Elteq!$F$8)","v":11.252097224678849}]
["REIKU-B","VMSVB-29/37",null,null,20,11.252068862361213,{"$f":"F1230*(1-Elteq!$F$8)","v":11.252068862361213}]
["REIKU-B","VMSVB-36/40",null,null,10,14.310319269428401,{"$f":"F1231*(1-Elteq!$F$8)","v":14.310319269428401}]
["REIKU-B","VMSVB-36/47",null,null,10,14.310257303163514,{"$f":"F1232*(1-Elteq!$F$8)","v":14.310257303163514}]
["REIKU-B","VMSVB-48/59",null,null,10,20.658901661284748,{"$f":"F1233*(1-Elteq!$F$8)","v":20.658901661284748}]
["REIKU-B","VPARB-10G01",null,null,50,2.6065572364644094,{"$f":"F1234*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-B","VPARB-10M16",null,null,50,2.6065572364644094,{"$f":"F1235*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-B","VPARB-10M20",null,null,50,2.6065572364644094,{"$f":"F1236*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-B","VPARB-10P09",null,null,50,2.6065572364644094,{"$f":"F1237*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-B","VPARB-12G01",null,null,50,2.7097872260273559,{"$f":"F1238*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-B","VPARB-12M16",null,null,50,2.7097872260273559,{"$f":"F1239*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-B","VPARB-12M20",null,null,50,2.7097872260273559,{"$f":"F1240*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-B","VPARB-12P11",null,null,50,2.6323647338551464,{"$f":"F1241*(1-Elteq!$F$8)","v":2.6323647338551464}]
["REIKU-B","VPARB-17G02",null,null,50,2.7097872260273559,{"$f":"F1242*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-B","VPARB-17M20",null,null,50,2.7097872260273559,{"$f":"F1243*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-B","VPARB-17M25",null,null,50,2.7097872260273559,{"$f":"F1244*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-B","VPARB-17P16",null,null,50,2.7097872260273559,{"$f":"F1245*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-B","VPARB-23G03",null,null,30,4.6840607764187148,{"$f":"F1246*(1-Elteq!$F$8)","v":4.6840607764187148}]
["REIKU-B","VPARB-23M25",null,null,50,4.6840607764187148,{"$f":"F1247*(1-Elteq!$F$8)","v":4.6840607764187148}]
["REIKU-B","VPARB-23M32",null,null,30,4.6840607764187148,{"$f":"F1248*(1-Elteq!$F$8)","v":4.6840607764187148}]
["REIKU-B","VPARB-23P21",null,null,30,4.6840607764187148,{"$f":"F1249*(1-Elteq!$F$8)","v":4.6840607764187148}]
["REIKU-B","VPARB-29G04",null,null,30,6.684141824200811,{"$f":"F1250*(1-Elteq!$F$8)","v":6.684141824200811}]
["REIKU-B","VPARB-29M32",null,null,30,6.684141824200811,{"$f":"F1251*(1-Elteq!$F$8)","v":6.684141824200811}]
["REIKU-B","VPARB-29M40",null,null,30,6.684141824200811,{"$f":"F1252*(1-Elteq!$F$8)","v":6.684141824200811}]
["REIKU-B","VPARB-29P29",null,null,30,6.684141824200811,{"$f":"F1253*(1-Elteq!$F$8)","v":6.684141824200811}]
["REIKU-B","VPARB-36G05",null,null,10,10.232672715427109,{"$f":"F1254*(1-Elteq!$F$8)","v":10.232672715427109}]
["REIKU-B","VPARB-36M40",null,null,10,10.232672715427109,{"$f":"F1255*(1-Elteq!$F$8)","v":10.232672715427109}]
["REIKU-B","VPARB-36M50",null,null,10,10.232672715427109,{"$f":"F1256*(1-Elteq!$F$8)","v":10.232672715427109}]
["REIKU-B","VPARB-36P36",null,null,10,10.232672715427109,{"$f":"F1257*(1-Elteq!$F$8)","v":10.232672715427109}]
["REIKU-B","VPARB-48G07",null,null,10,11.277876359751948,{"$f":"F1258*(1-Elteq!$F$8)","v":11.277876359751948}]
["REIKU-B","VPARB-48M50",null,null,10,11.277876359751948,{"$f":"F1259*(1-Elteq!$F$8)","v":11.277876359751948}]
["REIKU-B","VPARB-48M63",null,null,10,11.277876359751948,{"$f":"F1260*(1-Elteq!$F$8)","v":11.277876359751948}]
["REIKU-B","VPARB-48P48",null,null,10,11.277876359751948,{"$f":"F1261*(1-Elteq!$F$8)","v":11.277876359751948}]
["REIKU-B","VPAVB-10M16",null,null,50,2.7743059695041974,{"$f":"F1262*(1-Elteq!$F$8)","v":2.7743059695041974}]
["REIKU-B","VPAVB-10M20",null,null,50,2.8130172155903033,{"$f":"F1263*(1-Elteq!$F$8)","v":2.8130172155903033}]
["REIKU-B","VPAVB-10P09",null,null,50,2.7614022208088285,{"$f":"F1264*(1-Elteq!$F$8)","v":2.7614022208088285}]
["REIKU-B","VPAVB-12M16",null,null,50,2.8775359590671443,{"$f":"F1265*(1-Elteq!$F$8)","v":2.8775359590671443}]
["REIKU-B","VPAVB-12M20",null,null,50,2.9291509538486182,{"$f":"F1266*(1-Elteq!$F$8)","v":2.9291509538486182}]
["REIKU-B","VPAVB-12P11",null,null,50,2.8001134668949357,{"$f":"F1267*(1-Elteq!$F$8)","v":2.8001134668949357}]
["REIKU-B","VPAVB-17M20",null,null,50,2.9291509538486182,{"$f":"F1268*(1-Elteq!$F$8)","v":2.9291509538486182}]
["REIKU-B","VPAVB-17M25",null,null,50,2.9549584512393556,{"$f":"F1269*(1-Elteq!$F$8)","v":2.9549584512393556}]
["REIKU-B","VPAVB-17P16",null,null,50,2.9162472051532493,{"$f":"F1270*(1-Elteq!$F$8)","v":2.9162472051532493}]
["REIKU-B","VPAVB-23M25",null,null,30,4.9163282529353456,{"$f":"F1271*(1-Elteq!$F$8)","v":4.9163282529353456}]
["REIKU-B","VPAVB-23M32",null,null,30,5.0066544938029232,{"$f":"F1272*(1-Elteq!$F$8)","v":5.0066544938029232}]
["REIKU-B","VPAVB-23P21",null,null,30,4.9163282529353456,{"$f":"F1273*(1-Elteq!$F$8)","v":4.9163282529353456}]
["REIKU-B","VPAVB-29M32",null,null,30,7.0067355415850194,{"$f":"F1274*(1-Elteq!$F$8)","v":7.0067355415850194}]
["REIKU-B","VPAVB-29M40",null,null,30,7.1873880233201763,{"$f":"F1275*(1-Elteq!$F$8)","v":7.1873880233201763}]
["REIKU-B","VPAVB-29P29",null,null,30,7.0067355415850194,{"$f":"F1276*(1-Elteq!$F$8)","v":7.0067355415850194}]
["REIKU-B","VPAVB-36M40",null,null,10,10.735918914546478,{"$f":"F1277*(1-Elteq!$F$8)","v":10.735918914546478}]
["REIKU-B","VPAVB-36M50",null,null,10,10.955282642367742,{"$f":"F1278*(1-Elteq!$F$8)","v":10.955282642367742}]
["REIKU-B","VPAVB-36P36",null,null,10,10.63268892498353,{"$f":"F1279*(1-Elteq!$F$8)","v":10.63268892498353}]
["REIKU-B","VPAVB-48M50",null,null,10,12.000486286692574,{"$f":"F1280*(1-Elteq!$F$8)","v":12.000486286692574}]
["REIKU-B","VPAVB-48M63",null,null,10,12.21985001451384,{"$f":"F1281*(1-Elteq!$F$8)","v":12.21985001451384}]
["REIKU-B","VPAVB-48P48",null,null,10,11.755315061480575,{"$f":"F1282*(1-Elteq!$F$8)","v":11.755315061480575}]
["REIKU-B","VPBRB-10G01",null,null,50,2.6065572364644094,{"$f":"F1283*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-B","VPBRB-10M16",null,null,50,2.6065572364644094,{"$f":"F1284*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-B","VPBRB-10M20",null,null,50,2.6065572364644094,{"$f":"F1285*(1-Elteq!$F$8)","v":2.6065572364644094}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"VPBRB-10P09",null,null,50,2.6065572364644094,{"$f":"F1286*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-B","VPBRB-10P11",null,null,50,2.6839797286366194,{"$f":"F1287*(1-Elteq!$F$8)","v":2.6839797286366194}]
["REIKU-B","VPBRB-10P13",null,null,50,2.6839797286366194,{"$f":"F1288*(1-Elteq!$F$8)","v":2.6839797286366194}]
["REIKU-B","VPBRB-12G01",null,null,50,2.7097872260273559,{"$f":"F1289*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-B","VPBRB-12M16",null,null,50,2.7097872260273559,{"$f":"F1290*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-B","VPBRB-12M20",null,null,50,2.7097872260273559,{"$f":"F1291*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-B","VPBRB-12P11",null,null,50,2.6323647338551464,{"$f":"F1292*(1-Elteq!$F$8)","v":2.6323647338551464}]
["REIKU-B","VPBRB-12P13",null,null,50,2.7097872260273559,{"$f":"F1293*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-B","VPBRB-17G02",null,null,50,2.7097872260273559,{"$f":"F1294*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-B","VPBRB-17M20",null,null,50,2.7097872260273559,{"$f":"F1295*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-B","VPBRB-17M25",null,null,50,2.7097872260273559,{"$f":"F1296*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-B","VPBRB-17P13",null,null,50,2.7097872260273559,{"$f":"F1297*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-B","VPBRB-17P16",null,null,50,2.7097872260273559,{"$f":"F1298*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-B","VPBRB-23G03",null,null,30,4.6840607764187148,{"$f":"F1299*(1-Elteq!$F$8)","v":4.6840607764187148}]
["REIKU-B","VPBRB-23M25",null,null,30,4.6840607764187148,{"$f":"F1300*(1-Elteq!$F$8)","v":4.6840607764187148}]
["REIKU-B","VPBRB-23M32",null,null,30,4.6840607764187148,{"$f":"F1301*(1-Elteq!$F$8)","v":4.6840607764187148}]
["REIKU-B","VPBRB-23P21",null,null,30,4.6840607764187148,{"$f":"F1302*(1-Elteq!$F$8)","v":4.6840607764187148}]
["REIKU-B","VPBRB-29G04",null,null,30,6.684141824200811,{"$f":"F1303*(1-Elteq!$F$8)","v":6.684141824200811}]
["REIKU-B","VPBRB-29M32",null,null,30,6.684141824200811,{"$f":"F1304*(1-Elteq!$F$8)","v":6.684141824200811}]
["REIKU-B","VPBRB-29M40",null,null,30,6.684141824200811,{"$f":"F1305*(1-Elteq!$F$8)","v":6.684141824200811}]
["REIKU-B","VPBRB-29P29",null,null,30,6.684141824200811,{"$f":"F1306*(1-Elteq!$F$8)","v":6.684141824200811}]
["REIKU-B","VPBRB-36G05",null,null,10,10.232672715427109,{"$f":"F1307*(1-Elteq!$F$8)","v":10.232672715427109}]
["REIKU-B","VPBRB-36M40",null,null,10,10.232672715427109,{"$f":"F1308*(1-Elteq!$F$8)","v":10.232672715427109}]
["REIKU-B","VPBRB-36M50",null,null,10,10.232672715427109,{"$f":"F1309*(1-Elteq!$F$8)","v":10.232672715427109}]
["REIKU-B","VPBRB-36P36",null,null,10,10.232672715427109,{"$f":"F1310*(1-Elteq!$F$8)","v":10.232672715427109}]
["REIKU-B","VPBRB-48G07",null,null,10,11.277876359751948,{"$f":"F1311*(1-Elteq!$F$8)","v":11.277876359751948}]
["REIKU-B","VPBRB-48M50",null,null,10,11.277876359751948,{"$f":"F1312*(1-Elteq!$F$8)","v":11.277876359751948}]
["REIKU-B","VPBRB-48M63",null,null,10,11.277876359751948,{"$f":"F1313*(1-Elteq!$F$8)","v":11.277876359751948}]
["REIKU-B","VPBRB-48P48",null,null,10,11.277876359751948,{"$f":"F1314*(1-Elteq!$F$8)","v":11.277876359751948}]
["REIKU-B","VPBVB-10M16",null,null,50,2.7743059695041974,{"$f":"F1315*(1-Elteq!$F$8)","v":2.7743059695041974}]
["REIKU-B","VPBVB-10M20",null,null,50,2.8130172155903033,{"$f":"F1316*(1-Elteq!$F$8)","v":2.8130172155903033}]
["REIKU-B","VPBVB-10P09",null,null,50,2.7614022208088285,{"$f":"F1317*(1-Elteq!$F$8)","v":2.7614022208088285}]
["REIKU-B","VPBVB-10P11",null,null,50,2.8517284616764083,{"$f":"F1318*(1-Elteq!$F$8)","v":2.8517284616764083}]
["REIKU-B","VPBVB-10P13",null,null,50,2.8646322103717763,{"$f":"F1319*(1-Elteq!$F$8)","v":2.8646322103717763}]
["REIKU-B","VPBVB-12M16",null,null,50,2.8775359590671443,{"$f":"F1320*(1-Elteq!$F$8)","v":2.8775359590671443}]
["REIKU-B","VPBVB-12M20",null,null,50,2.9291509538486182,{"$f":"F1321*(1-Elteq!$F$8)","v":2.9291509538486182}]
["REIKU-B","VPBVB-12P11",null,null,50,2.8001134668949357,{"$f":"F1322*(1-Elteq!$F$8)","v":2.8001134668949357}]
["REIKU-B","VPBVB-12P13",null,null,50,2.8904397077625124,{"$f":"F1323*(1-Elteq!$F$8)","v":2.8904397077625124}]
["REIKU-B","VPBVB-17M20",null,null,50,2.9291509538486182,{"$f":"F1324*(1-Elteq!$F$8)","v":2.9291509538486182}]
["REIKU-B","VPBVB-17M25",null,null,50,2.9549584512393556,{"$f":"F1325*(1-Elteq!$F$8)","v":2.9549584512393556}]
["REIKU-B","VPBVB-17P13",null,null,50,2.8904397077625124,{"$f":"F1326*(1-Elteq!$F$8)","v":2.8904397077625124}]
["REIKU-B","VPBVB-17P16",null,null,50,2.9162472051532493,{"$f":"F1327*(1-Elteq!$F$8)","v":2.9162472051532493}]
["REIKU-B","VPBVB-23M25",null,null,30,4.9163282529353456,{"$f":"F1328*(1-Elteq!$F$8)","v":4.9163282529353456}]
["REIKU-B","VPBVB-23M32",null,null,30,5.0066544938029232,{"$f":"F1329*(1-Elteq!$F$8)","v":5.0066544938029232}]
["REIKU-B","VPBVB-23P21",null,null,30,4.9163282529353456,{"$f":"F1330*(1-Elteq!$F$8)","v":4.9163282529353456}]
["REIKU-B","VPBVB-29M32",null,null,30,7.0067355415850194,{"$f":"F1331*(1-Elteq!$F$8)","v":7.0067355415850194}]
["REIKU-B","VPBVB-29M40",null,null,30,7.1873880233201763,{"$f":"F1332*(1-Elteq!$F$8)","v":7.1873880233201763}]
["REIKU-B","VPBVB-29P29",null,null,30,7.0067355415850194,{"$f":"F1333*(1-Elteq!$F$8)","v":7.0067355415850194}]
["REIKU-B","VPBVB-36M40",null,null,10,10.735918914546478,{"$f":"F1334*(1-Elteq!$F$8)","v":10.735918914546478}]
["REIKU-B","VPBVB-36M50",null,null,10,10.955282642367742,{"$f":"F1335*(1-Elteq!$F$8)","v":10.955282642367742}]
["REIKU-B","VPBVB-36P36",null,null,10,10.63268892498353,{"$f":"F1336*(1-Elteq!$F$8)","v":10.63268892498353}]
["REIKU-B","VPBVB-48M50",null,null,10,12.000486286692574,{"$f":"F1337*(1-Elteq!$F$8)","v":12.000486286692574}]
["REIKU-B","VPBVB-48M63",null,null,10,12.21985001451384,{"$f":"F1338*(1-Elteq!$F$8)","v":12.21985001451384}]
["REIKU-B","VPBVB-48P48",null,null,10,11.755315061480575,{"$f":"F1339*(1-Elteq!$F$8)","v":11.755315061480575}]
["REIKU-B","VPGRB-10G00",null,null,50,1.4581236025766247,{"$f":"F1340*(1-Elteq!$F$8)","v":1.4581236025766247}]
["REIKU-B","VPGRB-10M12",null,null,50,1.4581236025766247,{"$f":"F1341*(1-Elteq!$F$8)","v":1.4581236025766247}]
["REIKU-B","VPGRB-10M16",null,null,50,1.4581236025766247,{"$f":"F1342*(1-Elteq!$F$8)","v":1.4581236025766247}]
["REIKU-B","VPGRB-10M16Z",null,null,30,3.6130496347031409,{"$f":"F1343*(1-Elteq!$F$8)","v":3.6130496347031409}]
["REIKU-B","VPGRB-10M20",null,null,50,1.4581236025766247,{"$f":"F1344*(1-Elteq!$F$8)","v":1.4581236025766247}]
["REIKU-B","VPGRB-10P07",null,null,50,1.4581236025766247,{"$f":"F1345*(1-Elteq!$F$8)","v":1.4581236025766247}]
["REIKU-B","VPGRB-10P09",null,null,50,1.4581236025766247,{"$f":"F1346*(1-Elteq!$F$8)","v":1.4581236025766247}]
["REIKU-B","VPGRB-10P11",null,null,50,1.4581236025766247,{"$f":"F1347*(1-Elteq!$F$8)","v":1.4581236025766247}]
["REIKU-B","VPGRB-10P13",null,null,50,1.4581236025766247,{"$f":"F1348*(1-Elteq!$F$8)","v":1.4581236025766247}]
["REIKU-B","VPGRB-12G01",null,null,50,1.4710273512719934,{"$f":"F1349*(1-Elteq!$F$8)","v":1.4710273512719934}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"VPGRB-12G02",null,null,50,1.4710273512719934,{"$f":"F1350*(1-Elteq!$F$8)","v":1.4710273512719934}]
["REIKU-B","VPGRB-12M16",null,null,50,1.4710273512719934,{"$f":"F1351*(1-Elteq!$F$8)","v":1.4710273512719934}]
["REIKU-B","VPGRB-12M16Z",null,null,30,3.7937021164382991,{"$f":"F1352*(1-Elteq!$F$8)","v":3.7937021164382991}]
["REIKU-B","VPGRB-12M20",null,null,50,1.4710273512719934,{"$f":"F1353*(1-Elteq!$F$8)","v":1.4710273512719934}]
["REIKU-B","VPGRB-12M20Z",null,null,30,3.7937021164382991,{"$f":"F1354*(1-Elteq!$F$8)","v":3.7937021164382991}]
["REIKU-B","VPGRB-12P09",null,null,50,1.4710273512719934,{"$f":"F1355*(1-Elteq!$F$8)","v":1.4710273512719934}]
["REIKU-B","VPGRB-12P11",null,null,50,1.4710273512719934,{"$f":"F1356*(1-Elteq!$F$8)","v":1.4710273512719934}]
["REIKU-B","VPGRB-12P13",null,null,50,1.4710273512719934,{"$f":"F1357*(1-Elteq!$F$8)","v":1.4710273512719934}]
["REIKU-B","VPGRB-17G02",null,null,50,1.4839310999673616,{"$f":"F1358*(1-Elteq!$F$8)","v":1.4839310999673616}]
["REIKU-B","VPGRB-17M20",null,null,50,1.4839310999673616,{"$f":"F1359*(1-Elteq!$F$8)","v":1.4839310999673616}]
["REIKU-B","VPGRB-17M20Z",null,null,30,4.5163120433789263,{"$f":"F1360*(1-Elteq!$F$8)","v":4.5163120433789263}]
["REIKU-B","VPGRB-17M25",null,null,50,1.4839310999673616,{"$f":"F1361*(1-Elteq!$F$8)","v":1.4839310999673616}]
["REIKU-B","VPGRB-17M32",null,null,50,1.5742573408349396,{"$f":"F1362*(1-Elteq!$F$8)","v":1.5742573408349396}]
["REIKU-B","VPGRB-17P11",null,null,50,1.4839310999673616,{"$f":"F1363*(1-Elteq!$F$8)","v":1.4839310999673616}]
["REIKU-B","VPGRB-17P13",null,null,50,1.4839310999673616,{"$f":"F1364*(1-Elteq!$F$8)","v":1.4839310999673616}]
["REIKU-B","VPGRB-17P16",null,null,50,1.4839310999673616,{"$f":"F1365*(1-Elteq!$F$8)","v":1.4839310999673616}]
["REIKU-B","VPGRB-17P21",null,null,50,1.9484660530006226,{"$f":"F1366*(1-Elteq!$F$8)","v":1.9484660530006226}]
["REIKU-B","VPGRB-23G03",null,null,30,2.4517122521199881,{"$f":"F1367*(1-Elteq!$F$8)","v":2.4517122521199881}]
["REIKU-B","VPGRB-23M25",null,null,30,2.4517122521199881,{"$f":"F1368*(1-Elteq!$F$8)","v":2.4517122521199881}]
["REIKU-B","VPGRB-23M25Z",null,null,30,5.4711894468361866,{"$f":"F1369*(1-Elteq!$F$8)","v":5.4711894468361866}]
["REIKU-B","VPGRB-23M32",null,null,30,2.5162309955968301,{"$f":"F1370*(1-Elteq!$F$8)","v":2.5162309955968301}]
["REIKU-B","VPGRB-23P16",null,null,50,2.4517122521199881,{"$f":"F1371*(1-Elteq!$F$8)","v":2.4517122521199881}]
["REIKU-B","VPGRB-23P21",null,null,30,2.4517122521199881,{"$f":"F1372*(1-Elteq!$F$8)","v":2.4517122521199881}]
["REIKU-B","VPGRB-29G04",null,null,30,3.1743221790606166,{"$f":"F1373*(1-Elteq!$F$8)","v":3.1743221790606166}]
["REIKU-B","VPGRB-29M32",null,null,30,3.1743221790606166,{"$f":"F1374*(1-Elteq!$F$8)","v":3.1743221790606166}]
["REIKU-B","VPGRB-29M32Z",null,null,20,7.2390030181016529,{"$f":"F1375*(1-Elteq!$F$8)","v":7.2390030181016529}]
["REIKU-B","VPGRB-29M40",null,null,30,3.1743221790606166,{"$f":"F1376*(1-Elteq!$F$8)","v":3.1743221790606166}]
["REIKU-B","VPGRB-29P29",null,null,30,3.1743221790606166,{"$f":"F1377*(1-Elteq!$F$8)","v":3.1743221790606166}]
["REIKU-B","VPGRB-36G05",null,null,10,5.4066707033593433,{"$f":"F1378*(1-Elteq!$F$8)","v":5.4066707033593433}]
["REIKU-B","VPGRB-36M40",null,null,10,5.4066707033593433,{"$f":"F1379*(1-Elteq!$F$8)","v":5.4066707033593433}]
["REIKU-B","VPGRB-36M40Z",null,null,10,13.626358622308985,{"$f":"F1380*(1-Elteq!$F$8)","v":13.626358622308985}]
["REIKU-B","VPGRB-36M50",null,null,10,5.4066707033593433,{"$f":"F1381*(1-Elteq!$F$8)","v":5.4066707033593433}]
["REIKU-B","VPGRB-36P29",null,null,10,5.4066707033593433,{"$f":"F1382*(1-Elteq!$F$8)","v":5.4066707033593433}]
["REIKU-B","VPGRB-36P36",null,null,10,5.4066707033593433,{"$f":"F1383*(1-Elteq!$F$8)","v":5.4066707033593433}]
["REIKU-B","VPGRB-48G06",null,null,10,6.9938317928896518,{"$f":"F1384*(1-Elteq!$F$8)","v":6.9938317928896518}]
["REIKU-B","VPGRB-48G07",null,null,10,6.9938317928896518,{"$f":"F1385*(1-Elteq!$F$8)","v":6.9938317928896518}]
["REIKU-B","VPGRB-48M50",null,null,10,6.9938317928896518,{"$f":"F1386*(1-Elteq!$F$8)","v":6.9938317928896518}]
["REIKU-B","VPGRB-48M63",null,null,10,6.9938317928896518,{"$f":"F1387*(1-Elteq!$F$8)","v":6.9938317928896518}]
["REIKU-B","VPGRB-48M63Z",null,null,10,15.639343418786451,{"$f":"F1388*(1-Elteq!$F$8)","v":15.639343418786451}]
["REIKU-B","VPGRB-48P42",null,null,10,6.9938317928896518,{"$f":"F1389*(1-Elteq!$F$8)","v":6.9938317928896518}]
["REIKU-B","VPGRB-48P48",null,null,10,6.9938317928896518,{"$f":"F1390*(1-Elteq!$F$8)","v":6.9938317928896518}]
["REIKU-B","VPGVB-10M12",null,null,50,1.6129685869210446,{"$f":"F1391*(1-Elteq!$F$8)","v":1.6129685869210446}]
["REIKU-B","VPGVB-10M16",null,null,50,1.6258723356164138,{"$f":"F1392*(1-Elteq!$F$8)","v":1.6258723356164138}]
["REIKU-B","VPGVB-10M20",null,null,50,1.6645835817025187,{"$f":"F1393*(1-Elteq!$F$8)","v":1.6645835817025187}]
["REIKU-B","VPGVB-10P07",null,null,50,1.6129685869210446,{"$f":"F1394*(1-Elteq!$F$8)","v":1.6129685869210446}]
["REIKU-B","VPGVB-10P09",null,null,50,1.6129685869210446,{"$f":"F1395*(1-Elteq!$F$8)","v":1.6129685869210446}]
["REIKU-B","VPGVB-10P11",null,null,50,1.6258723356164138,{"$f":"F1396*(1-Elteq!$F$8)","v":1.6258723356164138}]
["REIKU-B","VPGVB-10P13",null,null,50,1.638776084311782,{"$f":"F1397*(1-Elteq!$F$8)","v":1.638776084311782}]
["REIKU-B","VPGVB-10S15",null,null,50,1.6258723356164138,{"$f":"F1398*(1-Elteq!$F$8)","v":1.6258723356164138}]
["REIKU-B","VPGVB-12M16",null,null,50,1.638776084311782,{"$f":"F1399*(1-Elteq!$F$8)","v":1.638776084311782}]
["REIKU-B","VPGVB-12M20",null,null,50,1.6774873303978866,{"$f":"F1400*(1-Elteq!$F$8)","v":1.6774873303978866}]
["REIKU-B","VPGVB-12P09",null,null,50,1.6258723356164138,{"$f":"F1401*(1-Elteq!$F$8)","v":1.6258723356164138}]
["REIKU-B","VPGVB-12P11",null,null,50,1.638776084311782,{"$f":"F1402*(1-Elteq!$F$8)","v":1.638776084311782}]
["REIKU-B","VPGVB-12P13",null,null,50,1.65167983300715,{"$f":"F1403*(1-Elteq!$F$8)","v":1.65167983300715}]
["REIKU-B","VPGVB-12S19",null,null,50,1.638776084311782,{"$f":"F1404*(1-Elteq!$F$8)","v":1.638776084311782}]
["REIKU-B","VPGVB-17M20",null,null,50,1.6903910790932555,{"$f":"F1405*(1-Elteq!$F$8)","v":1.6903910790932555}]
["REIKU-B","VPGVB-17M25",null,null,50,1.7161985764839915,{"$f":"F1406*(1-Elteq!$F$8)","v":1.7161985764839915}]
["REIKU-B","VPGVB-17M32",null,null,50,1.9097548069145172,{"$f":"F1407*(1-Elteq!$F$8)","v":1.9097548069145172}]
["REIKU-B","VPGVB-17P11",null,null,50,1.65167983300715,{"$f":"F1408*(1-Elteq!$F$8)","v":1.65167983300715}]
["REIKU-B","VPGVB-17P13",null,null,50,1.6645835817025187,{"$f":"F1409*(1-Elteq!$F$8)","v":1.6645835817025187}]
["REIKU-B","VPGVB-17P16",null,null,50,1.6774873303978866,{"$f":"F1410*(1-Elteq!$F$8)","v":1.6774873303978866}]
["REIKU-B","VPGVB-17P21",null,null,50,2.1807335295172532,{"$f":"F1411*(1-Elteq!$F$8)","v":2.1807335295172532}]
["REIKU-B","VPGVB-17S22",null,null,50,1.6903910790932555,{"$f":"F1412*(1-Elteq!$F$8)","v":1.6903910790932555}]
["REIKU-B","VPGVB-23M25",null,null,30,2.6839797286366194,{"$f":"F1413*(1-Elteq!$F$8)","v":2.6839797286366194}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"VPGVB-23M32",null,null,30,2.8388247129810407,{"$f":"F1414*(1-Elteq!$F$8)","v":2.8388247129810407}]
["REIKU-B","VPGVB-23P16",null,null,50,2.6452684825505144,{"$f":"F1415*(1-Elteq!$F$8)","v":2.6452684825505144}]
["REIKU-B","VPGVB-23P21",null,null,30,2.6839797286366194,{"$f":"F1416*(1-Elteq!$F$8)","v":2.6839797286366194}]
["REIKU-B","VPGVB-23S28",null,null,30,2.7097872260273559,{"$f":"F1417*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-B","VPGVB-23S32",null,null,30,2.7097872260273559,{"$f":"F1418*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-B","VPGVB-29M32",null,null,30,3.5098196451401935,{"$f":"F1419*(1-Elteq!$F$8)","v":3.5098196451401935}]
["REIKU-B","VPGVB-29M40",null,null,30,3.6775683781799819,{"$f":"F1420*(1-Elteq!$F$8)","v":3.6775683781799819}]
["REIKU-B","VPGVB-29P29",null,null,30,3.5098196451401935,{"$f":"F1421*(1-Elteq!$F$8)","v":3.5098196451401935}]
["REIKU-B","VPGVB-29S37",null,null,30,3.5227233938355633,{"$f":"F1422*(1-Elteq!$F$8)","v":3.5227233938355633}]
["REIKU-B","VPGVB-29S40",null,null,30,3.5227233938355633,{"$f":"F1423*(1-Elteq!$F$8)","v":3.5227233938355633}]
["REIKU-B","VPGVB-36M40",null,null,10,5.9099169024787113,{"$f":"F1424*(1-Elteq!$F$8)","v":5.9099169024787113}]
["REIKU-B","VPGVB-36M50",null,null,10,6.1292806302999709,{"$f":"F1425*(1-Elteq!$F$8)","v":6.1292806302999709}]
["REIKU-B","VPGVB-36P29",null,null,10,5.7421681694389211,{"$f":"F1426*(1-Elteq!$F$8)","v":5.7421681694389211}]
["REIKU-B","VPGVB-36P36",null,null,10,5.8066869129157617,{"$f":"F1427*(1-Elteq!$F$8)","v":5.8066869129157617}]
["REIKU-B","VPGVB-48M50",null,null,10,7.7164417198302804,{"$f":"F1428*(1-Elteq!$F$8)","v":7.7164417198302804}]
["REIKU-B","VPGVB-48M63",null,null,10,7.9358054476515418,{"$f":"F1429*(1-Elteq!$F$8)","v":7.9358054476515418}]
["REIKU-B","VPGVB-48P42",null,null,10,8.0003241911283833,{"$f":"F1430*(1-Elteq!$F$8)","v":8.0003241911283833}]
["REIKU-B","VPGVB-48P48",null,null,10,7.471270494618282,{"$f":"F1431*(1-Elteq!$F$8)","v":7.471270494618282}]
["REIKU-B","VPHOB-12",null,null,50,1.3161823669275732,{"$f":"F1432*(1-Elteq!$F$8)","v":1.3161823669275732}]
["REIKU-B","VPHOB-17",null,null,50,2.1420222834311482,{"$f":"F1433*(1-Elteq!$F$8)","v":2.1420222834311482}]
["REIKU-B","VPHOB-23",null,null,20,2.6581722312458824,{"$f":"F1434*(1-Elteq!$F$8)","v":2.6581722312458824}]
["REIKU-B","VPHOB-29",null,null,20,3.2517446712328275,{"$f":"F1435*(1-Elteq!$F$8)","v":3.2517446712328275}]
["REIKU-B","VPHOB-36",null,null,20,5.8453981590018671,{"$f":"F1436*(1-Elteq!$F$8)","v":5.8453981590018671}]
["REIKU-B","VPHOB-42",null,null,20,6.0869909076877127,{"$f":"F1437*(1-Elteq!$F$8)","v":6.0869909076877127}]
["REIKU-B","VPHOB-48",null,null,20,6.8002755624591265,{"$f":"F1438*(1-Elteq!$F$8)","v":6.8002755624591265}]
["REIKU-B","VPIRB-10M121",null,null,50,2.0904072886496752,{"$f":"F1439*(1-Elteq!$F$8)","v":2.0904072886496752}]
["REIKU-B","VPIRB-10M16",null,null,50,2.0904072886496752,{"$f":"F1440*(1-Elteq!$F$8)","v":2.0904072886496752}]
["REIKU-B","VPIRB-10P07",null,null,50,2.0904072886496752,{"$f":"F1441*(1-Elteq!$F$8)","v":2.0904072886496752}]
["REIKU-B","VPIRB-10P09",null,null,50,2.0904072886496752,{"$f":"F1442*(1-Elteq!$F$8)","v":2.0904072886496752}]
["REIKU-B","VPIRB-10U05",null,null,50,2.464616000815357,{"$f":"F1443*(1-Elteq!$F$8)","v":2.464616000815357}]
["REIKU-B","VPIRB-10U07",null,null,50,2.464616000815357,{"$f":"F1444*(1-Elteq!$F$8)","v":2.464616000815357}]
["REIKU-B","VPIRB-12M16",null,null,50,2.1291185347357797,{"$f":"F1445*(1-Elteq!$F$8)","v":2.1291185347357797}]
["REIKU-B","VPIRB-12M20",null,null,50,2.1291185347357797,{"$f":"F1446*(1-Elteq!$F$8)","v":2.1291185347357797}]
["REIKU-B","VPIRB-12P11",null,null,50,2.1291185347357797,{"$f":"F1447*(1-Elteq!$F$8)","v":2.1291185347357797}]
["REIKU-B","VPIRB-12P13",null,null,50,2.1291185347357797,{"$f":"F1448*(1-Elteq!$F$8)","v":2.1291185347357797}]
["REIKU-B","VPIRB-12U05",null,null,50,2.5420384929875666,{"$f":"F1449*(1-Elteq!$F$8)","v":2.5420384929875666}]
["REIKU-B","VPIRB-12U06",null,null,50,2.5420384929875666,{"$f":"F1450*(1-Elteq!$F$8)","v":2.5420384929875666}]
["REIKU-B","VPIRB-12U07",null,null,50,2.5420384929875666,{"$f":"F1451*(1-Elteq!$F$8)","v":2.5420384929875666}]
["REIKU-B","VPIRB-12U09",null,null,50,2.5420384929875666,{"$f":"F1452*(1-Elteq!$F$8)","v":2.5420384929875666}]
["REIKU-B","VPIRB-12U10",null,null,50,2.5420384929875666,{"$f":"F1453*(1-Elteq!$F$8)","v":2.5420384929875666}]
["REIKU-B","VPIRB-17M20",null,null,50,2.2065410269079901,{"$f":"F1454*(1-Elteq!$F$8)","v":2.2065410269079901}]
["REIKU-B","VPIRB-17M25",null,null,50,2.2065410269079901,{"$f":"F1455*(1-Elteq!$F$8)","v":2.2065410269079901}]
["REIKU-B","VPIRB-17P13",null,null,50,2.2065410269079901,{"$f":"F1456*(1-Elteq!$F$8)","v":2.2065410269079901}]
["REIKU-B","VPIRB-17P16",null,null,50,2.2065410269079901,{"$f":"F1457*(1-Elteq!$F$8)","v":2.2065410269079901}]
["REIKU-B","VPIRB-17U07",null,null,50,2.6194609851597779,{"$f":"F1458*(1-Elteq!$F$8)","v":2.6194609851597779}]
["REIKU-B","VPIRB-17U09",null,null,50,2.6194609851597779,{"$f":"F1459*(1-Elteq!$F$8)","v":2.6194609851597779}]
["REIKU-B","VPIRB-17U10",null,null,50,2.6194609851597779,{"$f":"F1460*(1-Elteq!$F$8)","v":2.6194609851597779}]
["REIKU-B","VPIRB-17U11",null,null,50,2.6194609851597779,{"$f":"F1461*(1-Elteq!$F$8)","v":2.6194609851597779}]
["REIKU-B","VPIRB-17U14",null,null,50,2.6194609851597779,{"$f":"F1462*(1-Elteq!$F$8)","v":2.6194609851597779}]
["REIKU-B","VPIRB-17U17",null,null,50,2.6194609851597779,{"$f":"F1463*(1-Elteq!$F$8)","v":2.6194609851597779}]
["REIKU-B","VPIRB-23M25",null,null,30,4.5292157920742966,{"$f":"F1464*(1-Elteq!$F$8)","v":4.5292157920742966}]
["REIKU-B","VPIRB-23M32",null,null,30,4.5293102989558847,{"$f":"F1465*(1-Elteq!$F$8)","v":4.5293102989558847}]
["REIKU-B","VPIRB-23P21",null,null,30,4.5292157920742966,{"$f":"F1466*(1-Elteq!$F$8)","v":4.5292157920742966}]
["REIKU-B","VPIRB-23U14",null,null,30,5.4840931955315542,{"$f":"F1467*(1-Elteq!$F$8)","v":5.4840931955315542}]
["REIKU-B","VPIRB-23U17",null,null,30,5.4840931955315542,{"$f":"F1468*(1-Elteq!$F$8)","v":5.4840931955315542}]
["REIKU-B","VPIRB-23U18",null,null,30,5.4840931955315542,{"$f":"F1469*(1-Elteq!$F$8)","v":5.4840931955315542}]
["REIKU-B","VPIRB-29M32",null,null,30,7.768056714611757,{"$f":"F1470*(1-Elteq!$F$8)","v":7.768056714611757}]
["REIKU-B","VPIRB-29M40",null,null,30,7.7679821709365662,{"$f":"F1471*(1-Elteq!$F$8)","v":7.7679821709365662}]
["REIKU-B","VPIRB-29P29",null,null,30,7.768056714611757,{"$f":"F1472*(1-Elteq!$F$8)","v":7.768056714611757}]
["REIKU-B","VPIRB-29U24",null,null,30,9.3294103067513241,{"$f":"F1473*(1-Elteq!$F$8)","v":9.3294103067513241}]
["REIKU-B","VPIRB-36M40",null,null,10,8.5035703902477469,{"$f":"F1474*(1-Elteq!$F$8)","v":8.5035703902477469}]
["REIKU-B","VPIRB-36M50",null,null,10,8.5035781356397209,{"$f":"F1475*(1-Elteq!$F$8)","v":8.5035781356397209}]
["REIKU-B","VPIRB-36P36",null,null,10,8.5035703902477469,{"$f":"F1476*(1-Elteq!$F$8)","v":8.5035703902477469}]
["REIKU-B","VPIRB-48M50",null,null,10,15.381268444879082,{"$f":"F1477*(1-Elteq!$F$8)","v":15.381268444879082}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-B"},"VPIRB-48M63",null,null,10,15.381236960090622,{"$f":"F1478*(1-Elteq!$F$8)","v":15.381236960090622}]
["REIKU-B","VPIRB-48P48",null,null,10,15.381268444879082,{"$f":"F1479*(1-Elteq!$F$8)","v":15.381268444879082}]
["REIKU-B","VPIVB-36M40",null,null,10,9.0067829979237199,{"$f":"F1480*(1-Elteq!$F$8)","v":9.0067829979237199}]
["REIKU-B","VPSRB-10M12",null,null,50,3.2646484199281942,{"$f":"F1481*(1-Elteq!$F$8)","v":3.2646484199281942}]
["REIKU-B","VPSRB-10M16",null,null,50,3.2646484199281942,{"$f":"F1482*(1-Elteq!$F$8)","v":3.2646484199281942}]
["REIKU-B","VPSRB-10M20",null,null,50,3.2646484199281942,{"$f":"F1483*(1-Elteq!$F$8)","v":3.2646484199281942}]
["REIKU-B","VPSRB-12M20",null,null,50,3.380782158186511,{"$f":"F1484*(1-Elteq!$F$8)","v":3.380782158186511}]
["REIKU-B","VPSVB-10M12",null,null,50,3.4194934042726155,{"$f":"F1485*(1-Elteq!$F$8)","v":3.4194934042726155}]
["REIKU-B","VPSVB-10M16",null,null,50,3.4453009016633525,{"$f":"F1486*(1-Elteq!$F$8)","v":3.4453009016633525}]
["REIKU-B","VPSVB-10M20",null,null,50,3.4840121477494579,{"$f":"F1487*(1-Elteq!$F$8)","v":3.4840121477494579}]
["REIKU-B","VPSVB-12M20",null,null,50,3.6001458860077729,{"$f":"F1488*(1-Elteq!$F$8)","v":3.6001458860077729}]
["REIKU-B","ZKDRB-42",null,null,10,1.3161645178784107,{"$f":"F1489*(1-Elteq!$F$8)","v":1.3161645178784107}]
["REIKU-B","ZKDRB-52",null,null,10,1.3161645178784107,{"$f":"F1490*(1-Elteq!$F$8)","v":1.3161645178784107}]
["REIKU-B","ZKDRB-70",null,null,10,1.3161823669275732,{"$f":"F1491*(1-Elteq!$F$8)","v":1.3161823669275732}]
["REIKU-B","ZKDRB-95",null,null,10,1.3161823669275732,{"$f":"F1492*(1-Elteq!$F$8)","v":1.3161823669275732}]
["REIKU-B","Variable REIKU distribution piece, Basic piece for sizes NW07-NW17",null,null,10,0.77422492172210156,{"$f":"F1493*(1-Elteq!$F$8)","v":0.77422492172210156}]
["REIKU-B","PA connector NW 07 without seal",null,null,1,0.85164741389431153,{"$f":"F1494*(1-Elteq!$F$8)","v":0.85164741389431153}]
["REIKU-B","PA connector NW 10 without seal",null,null,1,0.85164741389431153,{"$f":"F1495*(1-Elteq!$F$8)","v":0.85164741389431153}]
["REIKU-B","PA connector NW 12 without seal",null,null,1,0.85164741389431153,{"$f":"F1496*(1-Elteq!$F$8)","v":0.85164741389431153}]
["REIKU-B","PA connector NW 17 without seal",null,null,1,0.85164741389431153,{"$f":"F1497*(1-Elteq!$F$8)","v":0.85164741389431153}]
["REIKU-B","PA connector NW 07 with seal",null,null,1,1.0323649679656515,{"$f":"F1498*(1-Elteq!$F$8)","v":1.0323649679656515}]
["REIKU-B","PA connector NW 10 with seal",null,null,1,1.0451075925445323,{"$f":"F1499*(1-Elteq!$F$8)","v":1.0451075925445323}]
["REIKU-B","PA connector NW 12 with seal",null,null,1,1.0580625941997275,{"$f":"F1500*(1-Elteq!$F$8)","v":1.0580625941997275}]
["REIKU-B","PA connector NW 17 with seal",null,null,1,1.0710175958549228,{"$f":"F1501*(1-Elteq!$F$8)","v":1.0710175958549228}]
["REIKU-B","VP connector NW 07",null,null,1,1.2129523773646258,{"$f":"F1502*(1-Elteq!$F$8)","v":1.2129523773646258}]
["REIKU-B","VP connector NW 10",null,null,1,1.2258561260599941,{"$f":"F1503*(1-Elteq!$F$8)","v":1.2258561260599941}]
["REIKU-B","VP connector NW 12",null,null,1,1.2387598747553628,{"$f":"F1504*(1-Elteq!$F$8)","v":1.2387598747553628}]
["REIKU-B","VP connector NW 17",null,null,1,1.2516636234507308,{"$f":"F1505*(1-Elteq!$F$8)","v":1.2516636234507308}]
["REIKU-B","Basic piece for sizes NW23 till NW29, reduceable to NW07",null,null,10,1.7420060738747289,{"$f":"F1506*(1-Elteq!$F$8)","v":1.7420060738747289}]
["REIKU-B","P2 connector NW07 without seal",null,null,1,1.0710111417155741,{"$f":"F1507*(1-Elteq!$F$8)","v":1.0710111417155741}]
["REIKU-B","P2 connector NW10 without seal",null,null,1,1.0710111417155741,{"$f":"F1508*(1-Elteq!$F$8)","v":1.0710111417155741}]
["REIKU-B","P2 connector NW12 without seal",null,null,1,1.1355298851924154,{"$f":"F1509*(1-Elteq!$F$8)","v":1.1355298851924154}]
["REIKU-B","P2 connector NW17 without seal",null,null,1,1.1355298851924154,{"$f":"F1510*(1-Elteq!$F$8)","v":1.1355298851924154}]
["REIKU-B","P2 connector NW23 without seal",null,null,1,1.6258723356164138,{"$f":"F1511*(1-Elteq!$F$8)","v":1.6258723356164138}]
["REIKU-B","P2 connector NW29 without seal",null,null,1,1.65167983300715,{"$f":"F1512*(1-Elteq!$F$8)","v":1.65167983300715}]
["REIKU-B","P2 connector NW07 with seal",null,null,1,1.251744033659365,{"$f":"F1513*(1-Elteq!$F$8)","v":1.251744033659365}]
["REIKU-B","P2 connector NW10 with seal",null,null,1,1.2644866582382457,{"$f":"F1514*(1-Elteq!$F$8)","v":1.2644866582382457}]
["REIKU-B","P2 connector NW12 with seal",null,null,1,1.3419604033702828,{"$f":"F1515*(1-Elteq!$F$8)","v":1.3419604033702828}]
["REIKU-B","P2 connector NW17 with seal",null,null,1,1.3549154050254786,{"$f":"F1516*(1-Elteq!$F$8)","v":1.3549154050254786}]
["REIKU-B","P2 connector NW23 with seal",null,null,1,2.0387333719721483,{"$f":"F1517*(1-Elteq!$F$8)","v":2.0387333719721483}]
["REIKU-B","P2 connector NW29 with seal",null,null,1,2.1677561284518183,{"$f":"F1518*(1-Elteq!$F$8)","v":2.1677561284518183}]
["REIKU-B","V2 connector NW07",null,null,1,1.264567372146099,{"$f":"F1519*(1-Elteq!$F$8)","v":1.264567372146099}]
["REIKU-B","V2 connector NW10",null,null,1,1.2774711208414677,{"$f":"F1520*(1-Elteq!$F$8)","v":1.2774711208414677}]
["REIKU-B","V2 connector NW12",null,null,1,1.3677973617090466,{"$f":"F1521*(1-Elteq!$F$8)","v":1.3677973617090466}]
["REIKU-B","V2 connector NW17",null,null,1,1.3807011104044142,{"$f":"F1522*(1-Elteq!$F$8)","v":1.3807011104044142}]
["REIKU-B","V2 connector NW23",null,null,1,2.0645997912589382,{"$f":"F1523*(1-Elteq!$F$8)","v":2.0645997912589382}]
["REIKU-B","V2 connector NW29",null,null,1,2.2194447756033582,{"$f":"F1524*(1-Elteq!$F$8)","v":2.2194447756033582}]

{"sheet":"REIKU-G","index":6,"n_rows":978,"n_cols":7,"rows_kept":978,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["sheetname","Obj.kód šedá",null,"Popis","Balenie","Cena za ks alebo m","Cena za kus po zľave"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-G"},"PAAOG-07M101",null,null,50,2.3912867506472817,{"$f":"F5*(1-Elteq!$F$8)","v":2.3912867506472817}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-G"},"PAAOG-07M16",null,null,50,2.3912867506472817,{"$f":"F6*(1-Elteq!$F$8)","v":2.3912867506472817}]
["REIKU-G","PAAOG-07M20",null,null,50,2.3912867506472817,{"$f":"F7*(1-Elteq!$F$8)","v":2.3912867506472817}]
["REIKU-G","PAAOG-07P07",null,null,50,2.4259047547292516,{"$f":"F8*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-G","PAAOG-07P09",null,null,50,2.4259047547292516,{"$f":"F9*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-G","PAAOG-07P11",null,null,50,2.3912867506472817,{"$f":"F10*(1-Elteq!$F$8)","v":2.3912867506472817}]
["REIKU-G","PAAOB-07P13",null,null,50,2.3912867506472817,{"$f":"F11*(1-Elteq!$F$8)","v":2.3912867506472817}]
["REIKU-G","PAAOB-07P16",null,null,50,2.3912867506472817,{"$f":"F12*(1-Elteq!$F$8)","v":2.3912867506472817}]
["REIKU-G","PAAOG-10P09",null,null,50,2.4259047547292516,{"$f":"F13*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-G","PAAOG-12P11",null,null,50,2.4775197495107255,{"$f":"F14*(1-Elteq!$F$8)","v":2.4775197495107255}]
["REIKU-G","PAAOG-17P16",null,null,50,2.6065572364644094,{"$f":"F15*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-G","PAAOG-23P21",null,null,30,4.2969483155576649,{"$f":"F16*(1-Elteq!$F$8)","v":4.2969483155576649}]
["REIKU-G","PAAOG-29P29",null,null,30,6.2583181172536539,{"$f":"F17*(1-Elteq!$F$8)","v":6.2583181172536539}]
["REIKU-G","PAAVG-07P07",null,null,50,2.7614022208088285,{"$f":"F18*(1-Elteq!$F$8)","v":2.7614022208088285}]
["REIKU-G","PAAVG-07P09",null,null,50,2.7614022208088285,{"$f":"F19*(1-Elteq!$F$8)","v":2.7614022208088285}]
["REIKU-G","PAAVG-10P09",null,null,50,2.7743059695041974,{"$f":"F20*(1-Elteq!$F$8)","v":2.7743059695041974}]
["REIKU-G","PAAVG-12P11",null,null,50,2.8517284616764083,{"$f":"F21*(1-Elteq!$F$8)","v":2.8517284616764083}]
["REIKU-G","PAAVG-17P16",null,null,50,3.0323809434115661,{"$f":"F22*(1-Elteq!$F$8)","v":3.0323809434115661}]
["REIKU-G","PAAVG-23P21",null,null,30,4.9421357503260825,{"$f":"F23*(1-Elteq!$F$8)","v":4.9421357503260825}]
["REIKU-G","PAAVG-29P29",null,null,30,7.0970617824525961,{"$f":"F24*(1-Elteq!$F$8)","v":7.0970617824525961}]
["REIKU-G","PACSG",null,null,50,0.23226747651663035,{"$f":"F25*(1-Elteq!$F$8)","v":0.23226747651663035}]
["REIKU-G","PADSG-07/10",null,null,100,0.24517122521199883,{"$f":"F26*(1-Elteq!$F$8)","v":0.24517122521199883}]
["REIKU-G","PADSG-12",null,null,50,0.25807497390736728,{"$f":"F27*(1-Elteq!$F$8)","v":0.25807497390736728}]
["REIKU-G","PADSG-14/17",null,null,50,0.27097872260273559,{"$f":"F28*(1-Elteq!$F$8)","v":0.27097872260273559}]
["REIKU-G","PADSG-23",null,null,50,0.34840121477494562,{"$f":"F29*(1-Elteq!$F$8)","v":0.34840121477494562}]
["REIKU-G","PADSG-29",null,null,30,0.47743870172862929,{"$f":"F30*(1-Elteq!$F$8)","v":0.47743870172862929}]
["REIKU-G","PADSG-36",null,null,20,0.54195744520547118,{"$f":"F31*(1-Elteq!$F$8)","v":0.54195744520547118}]
["REIKU-G","PADSG-48",null,null,20,0.64518743476841811,{"$f":"F32*(1-Elteq!$F$8)","v":0.64518743476841811}]
["REIKU-G","PAFOG-07",null,null,50,1.0508895270304723,{"$f":"F33*(1-Elteq!$F$8)","v":1.0508895270304723}]
["REIKU-G","PAFOG-10",null,null,50,1.1702730906393146,{"$f":"F34*(1-Elteq!$F$8)","v":1.1702730906393146}]
["REIKU-G","PAFOG-12",null,null,50,1.3852813178624774,{"$f":"F35*(1-Elteq!$F$8)","v":1.3852813178624774}]
["REIKU-G","PAFOG-17",null,null,30,2.0516960425635697,{"$f":"F36*(1-Elteq!$F$8)","v":2.0516960425635697}]
["REIKU-G","PAFOG-23",null,null,30,3.3678784094911429,{"$f":"F37*(1-Elteq!$F$8)","v":3.3678784094911429}]
["REIKU-G","PAFOG-29",null,null,20,5.0453657398890277,{"$f":"F38*(1-Elteq!$F$8)","v":5.0453657398890277}]
["REIKU-G","PAFOG-36",null,null,10,7.4454629972275459,{"$f":"F39*(1-Elteq!$F$8)","v":7.4454629972275459}]
["REIKU-G","PAFOG-48",null,null,10,10.142346474559533,{"$f":"F40*(1-Elteq!$F$8)","v":10.142346474559533}]
["REIKU-G","PAFVG-17",null,null,30,2.6581722312458824,{"$f":"F41*(1-Elteq!$F$8)","v":2.6581722312458824}]
["REIKU-G","PAFVG-23",null,null,30,4.2582370694715594,{"$f":"F42*(1-Elteq!$F$8)","v":4.2582370694715594}]
["REIKU-G","PAFVG-29",null,null,20,6.1937993737768124,{"$f":"F43*(1-Elteq!$F$8)","v":6.1937993737768124}]
["REIKU-G","PAFVG-36",null,null,10,9.122950327625432,{"$f":"F44*(1-Elteq!$F$8)","v":9.122950327625432}]
["REIKU-G","PAFVG-48",null,null,10,12.335983752772155,{"$f":"F45*(1-Elteq!$F$8)","v":12.335983752772155}]
["REIKU-G","PAGMB-07S22",null,null,50,1.9226585556098852,{"$f":"F46*(1-Elteq!$F$8)","v":1.9226585556098852}]
["REIKU-G","PAGMB-11S22",null,null,50,2.0904072886496752,{"$f":"F47*(1-Elteq!$F$8)","v":2.0904072886496752}]
["REIKU-G","PAGMB-20S32",null,null,50,2.7024832173318645,{"$f":"F48*(1-Elteq!$F$8)","v":2.7024832173318645}]
["REIKU-G","PAGMB-25S32",null,null,25,2.7024832173318645,{"$f":"F49*(1-Elteq!$F$8)","v":2.7024832173318645}]
["REIKU-G","PAGMB-32S40",null,null,25,3.3720173477519197,{"$f":"F50*(1-Elteq!$F$8)","v":3.3720173477519197}]
["REIKU-G","PAGMB-M12",null,null,100,0.19355623043052539,{"$f":"F51*(1-Elteq!$F$8)","v":0.19355623043052539}]
["REIKU-G","PAGMB-M16",null,null,100,0.20645997912589376,{"$f":"F52*(1-Elteq!$F$8)","v":0.20645997912589376}]
["REIKU-G","PAGMB-M20",null,null,100,0.30968996868884069,{"$f":"F53*(1-Elteq!$F$8)","v":0.30968996868884069}]
["REIKU-G","PAGMB-M25",null,null,100,0.32259371738420906,{"$f":"F54*(1-Elteq!$F$8)","v":0.32259371738420906}]
["REIKU-G","PAGMB-M32",null,null,50,0.70970617824526017,{"$f":"F55*(1-Elteq!$F$8)","v":0.70970617824526017}]
["REIKU-G","PAGMB-M40",null,null,25,1.0322998956294691,{"$f":"F56*(1-Elteq!$F$8)","v":1.0322998956294691}]
["REIKU-G","PAGMB-M50",null,null,25,1.3548936130136779,{"$f":"F57*(1-Elteq!$F$8)","v":1.3548936130136779}]
["REIKU-G","PAGMB-M63",null,null,25,1.5226423460534666,{"$f":"F58*(1-Elteq!$F$8)","v":1.5226423460534666}]
["REIKU-G","PAGOG-07G00",null,null,50,1.0072988179496118,{"$f":"F59*(1-Elteq!$F$8)","v":1.0072988179496118}]
["REIKU-G","PAGOG-07M101",null,null,50,1.0072988179496118,{"$f":"F60*(1-Elteq!$F$8)","v":1.0072988179496118}]
["REIKU-G","PAGOG-07M12",null,null,50,1.0072988179496118,{"$f":"F61*(1-Elteq!$F$8)","v":1.0072988179496118}]
["REIKU-G","PAGOG-07M12Z",null,null,30,2.6065572364644094,{"$f":"F62*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-G","PAGOG-07M16",null,null,50,1.0072988179496118,{"$f":"F63*(1-Elteq!$F$8)","v":1.0072988179496118}]
["REIKU-G","PAGOG-07M20",null,null,50,1.0072988179496118,{"$f":"F64*(1-Elteq!$F$8)","v":1.0072988179496118}]
["REIKU-G","PAGOG-07P07",null,null,50,1.0072988179496118,{"$f":"F65*(1-Elteq!$F$8)","v":1.0072988179496118}]
["REIKU-G","PAGOG-07P07Z",null,null,30,2.6065572364644094,{"$f":"F66*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-G","PAGOG-07P09",null,null,50,1.0072988179496118,{"$f":"F67*(1-Elteq!$F$8)","v":1.0072988179496118}]
["REIKU-G","PAGOG-07P11",null,null,50,1.0072988179496118,{"$f":"F68*(1-Elteq!$F$8)","v":1.0072988179496118}]
["REIKU-G","PAGOG-07P13",null,null,50,1.0072988179496118,{"$f":"F69*(1-Elteq!$F$8)","v":1.0072988179496118}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-G"},"PAGOG-07S13",null,null,50,1.1604553633688508,{"$f":"F70*(1-Elteq!$F$8)","v":1.1604553633688508}]
["REIKU-G","PAGOG-10M12",null,null,50,1.1015489997460666,{"$f":"F71*(1-Elteq!$F$8)","v":1.1015489997460666}]
["REIKU-G","PAGOG-10M16",null,null,50,1.1015489997460666,{"$f":"F72*(1-Elteq!$F$8)","v":1.1015489997460666}]
["REIKU-G","PAGOG-10M16Z",null,null,30,3.1356109329745108,{"$f":"F73*(1-Elteq!$F$8)","v":3.1356109329745108}]
["REIKU-G","PAGOG-10M20",null,null,50,1.1015489997460666,{"$f":"F74*(1-Elteq!$F$8)","v":1.1015489997460666}]
["REIKU-G","PAGOG-10P07",null,null,50,1.0308613633987256,{"$f":"F75*(1-Elteq!$F$8)","v":1.0308613633987256}]
["REIKU-G","PAGOG-10P09",null,null,50,1.0308613633987256,{"$f":"F76*(1-Elteq!$F$8)","v":1.0308613633987256}]
["REIKU-G","PAGOG-10P09Z",null,null,30,2.8775359590671443,{"$f":"F77*(1-Elteq!$F$8)","v":2.8775359590671443}]
["REIKU-G","PAGOG-10P11",null,null,50,1.1015489997460666,{"$f":"F78*(1-Elteq!$F$8)","v":1.1015489997460666}]
["REIKU-G","PAGOG-10P13",null,null,50,1.1015489997460666,{"$f":"F79*(1-Elteq!$F$8)","v":1.1015489997460666}]
["REIKU-G","PAGOG-10S15",null,null,50,1.1722366360934076,{"$f":"F80*(1-Elteq!$F$8)","v":1.1722366360934076}]
["REIKU-G","PAGOG-12M16",null,null,50,1.1015489997460666,{"$f":"F81*(1-Elteq!$F$8)","v":1.1015489997460666}]
["REIKU-G","PAGOG-12M16Z",null,null,30,3.2904559173189316,{"$f":"F82*(1-Elteq!$F$8)","v":3.2904559173189316}]
["REIKU-G","PAGOG-12M20",null,null,50,1.1015489997460666,{"$f":"F83*(1-Elteq!$F$8)","v":1.1015489997460666}]
["REIKU-G","PAGOG-12M20Z",null,null,30,3.2904559173189316,{"$f":"F84*(1-Elteq!$F$8)","v":3.2904559173189316}]
["REIKU-G","PAGOG-12P09",null,null,50,1.1015489997460666,{"$f":"F85*(1-Elteq!$F$8)","v":1.1015489997460666}]
["REIKU-G","PAGOG-12P11",null,null,50,1.1015489997460666,{"$f":"F86*(1-Elteq!$F$8)","v":1.1015489997460666}]
["REIKU-G","PAGOG-12P11Z",null,null,30,2.9936696973254597,{"$f":"F87*(1-Elteq!$F$8)","v":2.9936696973254597}]
["REIKU-G","PAGOG-12P13",null,null,50,1.1015489997460666,{"$f":"F88*(1-Elteq!$F$8)","v":1.1015489997460666}]
["REIKU-G","PAGOG-12P13Z",null,null,30,3.0194771947161958,{"$f":"F89*(1-Elteq!$F$8)","v":3.0194771947161958}]
["REIKU-G","PAGOG-12S19",null,null,50,1.1840179088179645,{"$f":"F90*(1-Elteq!$F$8)","v":1.1840179088179645}]
["REIKU-G","PAGOG-17M20",null,null,50,1.1133302724706238,{"$f":"F91*(1-Elteq!$F$8)","v":1.1133302724706238}]
["REIKU-G","PAGOG-17M20Z",null,null,30,3.9098358546966128,{"$f":"F92*(1-Elteq!$F$8)","v":3.9098358546966128}]
["REIKU-G","PAGOG-17M25",null,null,50,1.1133302724706238,{"$f":"F93*(1-Elteq!$F$8)","v":1.1133302724706238}]
["REIKU-G","PAGOG-17M32",null,null,50,1.1133302724706238,{"$f":"F94*(1-Elteq!$F$8)","v":1.1133302724706238}]
["REIKU-G","PAGOG-17P11",null,null,50,1.1133302724706238,{"$f":"F95*(1-Elteq!$F$8)","v":1.1133302724706238}]
["REIKU-G","PAGOG-17P13",null,null,50,1.1133302724706238,{"$f":"F96*(1-Elteq!$F$8)","v":1.1133302724706238}]
["REIKU-G","PAGOG-17P16",null,null,50,1.1133302724706238,{"$f":"F97*(1-Elteq!$F$8)","v":1.1133302724706238}]
["REIKU-G","PAGOG-17P16Z",null,null,30,3.5614346399216661,{"$f":"F98*(1-Elteq!$F$8)","v":3.5614346399216661}]
["REIKU-G","PAGOG-17P21",null,null,50,1.7534460905048797,{"$f":"F99*(1-Elteq!$F$8)","v":1.7534460905048797}]
["REIKU-G","PAGOG-17S22",null,null,50,1.1957991815425215,{"$f":"F100*(1-Elteq!$F$8)","v":1.1957991815425215}]
["REIKU-G","PAGOG-23M25",null,null,30,1.7770086359539934,{"$f":"F101*(1-Elteq!$F$8)","v":1.7770086359539934}]
["REIKU-G","PAGOG-23M25Z",null,null,30,4.7614832685909265,{"$f":"F102*(1-Elteq!$F$8)","v":4.7614832685909265}]
["REIKU-G","PAGOG-23M32",null,null,30,1.7770086359539934,{"$f":"F103*(1-Elteq!$F$8)","v":1.7770086359539934}]
["REIKU-G","PAGOG-23P16",null,null,50,1.7887899086785501,{"$f":"F104*(1-Elteq!$F$8)","v":1.7887899086785501}]
["REIKU-G","PAGOG-23P21",null,null,30,1.7887899086785501,{"$f":"F105*(1-Elteq!$F$8)","v":1.7887899086785501}]
["REIKU-G","PAGOG-23P21Z",null,null,30,4.3743708077298731,{"$f":"F106*(1-Elteq!$F$8)","v":4.3743708077298731}]
["REIKU-G","PAGOG-23S28",null,null,30,2.1088478176956786,{"$f":"F107*(1-Elteq!$F$8)","v":2.1088478176956786}]
["REIKU-G","PAGOG-23S32",null,null,30,2.1088478176956786,{"$f":"F108*(1-Elteq!$F$8)","v":2.1088478176956786}]
["REIKU-G","PAGOG-29M32",null,null,30,2.3444732721868151,{"$f":"F109*(1-Elteq!$F$8)","v":2.3444732721868151}]
["REIKU-G","PAGOG-29M32Z",null,null,20,6.2841256146443927,{"$f":"F110*(1-Elteq!$F$8)","v":6.2841256146443927}]
["REIKU-G","PAGOG-29M40",null,null,30,2.3444732721868151,{"$f":"F111*(1-Elteq!$F$8)","v":2.3444732721868151}]
["REIKU-G","PAGOG-29P29",null,null,30,2.3444732721868151,{"$f":"F112*(1-Elteq!$F$8)","v":2.3444732721868151}]
["REIKU-G","PAGOG-29P29Z",null,null,20,5.8453981590018671,{"$f":"F113*(1-Elteq!$F$8)","v":5.8453981590018671}]
["REIKU-G","PAGOG-29S37",null,null,30,3.0808028174716195,{"$f":"F114*(1-Elteq!$F$8)","v":3.0808028174716195}]
["REIKU-G","PAGOG-29S40",null,null,30,3.0808028174716195,{"$f":"F115*(1-Elteq!$F$8)","v":3.0808028174716195}]
["REIKU-G","PAGOG-36M40",null,null,10,4.0036691808952414,{"$f":"F116*(1-Elteq!$F$8)","v":4.0036691808952414}]
["REIKU-G","PAGOG-36M40Z",null,null,10,11.832737553652786,{"$f":"F117*(1-Elteq!$F$8)","v":11.832737553652786}]
["REIKU-G","PAGOG-36M50",null,null,10,4.0036691808952414,{"$f":"F118*(1-Elteq!$F$8)","v":4.0036691808952414}]
["REIKU-G","PAGOG-36P29",null,null,10,4.0036691808952414,{"$f":"F119*(1-Elteq!$F$8)","v":4.0036691808952414}]
["REIKU-G","PAGOG-36P36",null,null,10,4.0036691808952414,{"$f":"F120*(1-Elteq!$F$8)","v":4.0036691808952414}]
["REIKU-G","PAGOG-36P36Z",null,null,10,11.832737553652786,{"$f":"F121*(1-Elteq!$F$8)","v":11.832737553652786}]
["REIKU-G","PAGOG-48M50",null,null,10,5.2112496351623179,{"$f":"F122*(1-Elteq!$F$8)","v":5.2112496351623179}]
["REIKU-G","PAGOG-48M63",null,null,10,5.2112496351623179,{"$f":"F123*(1-Elteq!$F$8)","v":5.2112496351623179}]
["REIKU-G","PAGOG-48M63Z",null,null,10,13.587647376222883,{"$f":"F124*(1-Elteq!$F$8)","v":13.587647376222883}]
["REIKU-G","PAGOG-48P42",null,null,10,5.2112496351623179,{"$f":"F125*(1-Elteq!$F$8)","v":5.2112496351623179}]
["REIKU-G","PAGOG-48P48",null,null,10,5.2112496351623179,{"$f":"F126*(1-Elteq!$F$8)","v":5.2112496351623179}]
["REIKU-G","PAGOG-48P48Z",null,null,10,13.587647376222883,{"$f":"F127*(1-Elteq!$F$8)","v":13.587647376222883}]
["REIKU-G","PAGOG-52",null,null,10,9.4642890887273463,{"$f":"F128*(1-Elteq!$F$8)","v":9.4642890887273463}]
["REIKU-G","PAGOG-70",null,null,10,10.471587906676957,{"$f":"F129*(1-Elteq!$F$8)","v":10.471587906676957}]
["REIKU-G","PAGOG-95",null,null,10,12.757154815240989,{"$f":"F130*(1-Elteq!$F$8)","v":12.757154815240989}]
["REIKU-G","PAGVG-07M101",null,null,50,1.4323161051858881,{"$f":"F131*(1-Elteq!$F$8)","v":1.4323161051858881}]
["REIKU-G","PAGVG-07M12",null,null,50,1.4452198538812562,{"$f":"F132*(1-Elteq!$F$8)","v":1.4452198538812562}]
["REIKU-G","PAGVG-07M12Z",null,null,30,2.9549584512393556,{"$f":"F133*(1-Elteq!$F$8)","v":2.9549584512393556}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-G"},"PAGVG-07M16",null,null,50,1.4581236025766247,{"$f":"F134*(1-Elteq!$F$8)","v":1.4581236025766247}]
["REIKU-G","PAGVG-07M20",null,null,50,1.4968348486627299,{"$f":"F135*(1-Elteq!$F$8)","v":1.4968348486627299}]
["REIKU-G","PAGVG-07P07",null,null,50,1.4452198538812562,{"$f":"F136*(1-Elteq!$F$8)","v":1.4452198538812562}]
["REIKU-G","PAGVG-07P07Z",null,null,30,2.9549584512393556,{"$f":"F137*(1-Elteq!$F$8)","v":2.9549584512393556}]
["REIKU-G","PAGVG-07P09",null,null,50,1.4452198538812562,{"$f":"F138*(1-Elteq!$F$8)","v":1.4452198538812562}]
["REIKU-G","PAGVG-07P11",null,null,50,1.4581236025766247,{"$f":"F139*(1-Elteq!$F$8)","v":1.4581236025766247}]
["REIKU-G","PAGVG-07P13",null,null,50,1.4839310999673616,{"$f":"F140*(1-Elteq!$F$8)","v":1.4839310999673616}]
["REIKU-G","PAGVG-10M12",null,null,50,1.5613535921395714,{"$f":"F141*(1-Elteq!$F$8)","v":1.5613535921395714}]
["REIKU-G","PAGVG-10M16",null,null,50,1.5742573408349396,{"$f":"F142*(1-Elteq!$F$8)","v":1.5742573408349396}]
["REIKU-G","PAGVG-10M16Z",null,null,30,3.5098196451401935,{"$f":"F143*(1-Elteq!$F$8)","v":3.5098196451401935}]
["REIKU-G","PAGVG-10M20",null,null,50,1.6129685869210446,{"$f":"F144*(1-Elteq!$F$8)","v":1.6129685869210446}]
["REIKU-G","PAGVG-10P07",null,null,50,1.4839310999673616,{"$f":"F145*(1-Elteq!$F$8)","v":1.4839310999673616}]
["REIKU-G","PAGVG-10P09",null,null,50,1.4839310999673616,{"$f":"F146*(1-Elteq!$F$8)","v":1.4839310999673616}]
["REIKU-G","PAGVG-10P09Z",null,null,30,3.238840922537459,{"$f":"F147*(1-Elteq!$F$8)","v":3.238840922537459}]
["REIKU-G","PAGVG-10P11",null,null,50,1.5742573408349396,{"$f":"F148*(1-Elteq!$F$8)","v":1.5742573408349396}]
["REIKU-G","PAGVG-10P13",null,null,50,1.5871610895303083,{"$f":"F149*(1-Elteq!$F$8)","v":1.5871610895303083}]
["REIKU-G","PAGVG-12M16",null,null,50,1.5871610895303083,{"$f":"F150*(1-Elteq!$F$8)","v":1.5871610895303083}]
["REIKU-G","PAGVG-12M16Z",null,null,30,3.6775683781799819,{"$f":"F151*(1-Elteq!$F$8)","v":3.6775683781799819}]
["REIKU-G","PAGVG-12M20",null,null,50,1.6258723356164138,{"$f":"F152*(1-Elteq!$F$8)","v":1.6258723356164138}]
["REIKU-G","PAGVG-12M20Z",null,null,30,3.7162796242660856,{"$f":"F153*(1-Elteq!$F$8)","v":3.7162796242660856}]
["REIKU-G","PAGVG-12P09",null,null,50,1.5742573408349396,{"$f":"F154*(1-Elteq!$F$8)","v":1.5742573408349396}]
["REIKU-G","PAGVG-12P11",null,null,50,1.5871610895303083,{"$f":"F155*(1-Elteq!$F$8)","v":1.5871610895303083}]
["REIKU-G","PAGVG-12P11Z",null,null,30,3.3678784094911429,{"$f":"F156*(1-Elteq!$F$8)","v":3.3678784094911429}]
["REIKU-G","PAGVG-12P13",null,null,50,1.6000648382256766,{"$f":"F157*(1-Elteq!$F$8)","v":1.6000648382256766}]
["REIKU-G","PAGVG-12P13Z",null,null,30,3.4065896555772461,{"$f":"F158*(1-Elteq!$F$8)","v":3.4065896555772461}]
["REIKU-G","PAGVG-17M20",null,null,50,1.65167983300715,{"$f":"F159*(1-Elteq!$F$8)","v":1.65167983300715}]
["REIKU-G","PAGVG-17M20Z",null,null,30,4.3485633103391379,{"$f":"F160*(1-Elteq!$F$8)","v":4.3485633103391379}]
["REIKU-G","PAGVG-17M25",null,null,50,1.6774873303978866,{"$f":"F161*(1-Elteq!$F$8)","v":1.6774873303978866}]
["REIKU-G","PAGVG-17M32",null,null,50,1.7678135712654652,{"$f":"F162*(1-Elteq!$F$8)","v":1.7678135712654652}]
["REIKU-G","PAGVG-17P11",null,null,50,1.6774873303978866,{"$f":"F163*(1-Elteq!$F$8)","v":1.6774873303978866}]
["REIKU-G","PAGVG-17P13",null,null,50,1.6258723356164138,{"$f":"F164*(1-Elteq!$F$8)","v":1.6258723356164138}]
["REIKU-G","PAGVG-17P16",null,null,50,1.638776084311782,{"$f":"F165*(1-Elteq!$F$8)","v":1.638776084311782}]
["REIKU-G","PAGVG-17P16Z",null,null,30,3.9872583468688241,{"$f":"F166*(1-Elteq!$F$8)","v":3.9872583468688241}]
["REIKU-G","PAGVG-17P21",null,null,50,2.3613860112524097,{"$f":"F167*(1-Elteq!$F$8)","v":2.3613860112524097}]
["REIKU-G","PAGVG-23M25",null,null,30,2.5807497390736724,{"$f":"F168*(1-Elteq!$F$8)","v":2.5807497390736724}]
["REIKU-G","PAGVG-23M25Z",null,null,30,5.4066707033593433,{"$f":"F169*(1-Elteq!$F$8)","v":5.4066707033593433}]
["REIKU-G","PAGVG-23M32",null,null,30,2.6710759799412513,{"$f":"F170*(1-Elteq!$F$8)","v":2.6710759799412513}]
["REIKU-G","PAGVG-23P16",null,null,50,2.5549422416829355,{"$f":"F171*(1-Elteq!$F$8)","v":2.5549422416829355}]
["REIKU-G","PAGVG-23P21",null,null,30,2.5936534877690405,{"$f":"F172*(1-Elteq!$F$8)","v":2.5936534877690405}]
["REIKU-G","PAGVG-23P21Z",null,null,30,5.0324619911936601,{"$f":"F173*(1-Elteq!$F$8)","v":5.0324619911936601}]
["REIKU-G","PAGVG-29M32",null,null,30,3.3936859068818794,{"$f":"F174*(1-Elteq!$F$8)","v":3.3936859068818794}]
["REIKU-G","PAGVG-29M32Z",null,null,20,7.1228692798433322,{"$f":"F175*(1-Elteq!$F$8)","v":7.1228692798433322}]
["REIKU-G","PAGVG-29M40",null,null,30,3.5743383886170359,{"$f":"F176*(1-Elteq!$F$8)","v":3.5743383886170359}]
["REIKU-G","PAGVG-29P29",null,null,30,3.3936859068818794,{"$f":"F177*(1-Elteq!$F$8)","v":3.3936859068818794}]
["REIKU-G","PAGVG-29P29Z",null,null,20,6.6970455728961822,{"$f":"F178*(1-Elteq!$F$8)","v":6.6970455728961822}]
["REIKU-G","PAGVG-36M40",null,null,10,5.6647456772667102,{"$f":"F179*(1-Elteq!$F$8)","v":5.6647456772667102}]
["REIKU-G","PAGVG-36M40Z",null,null,10,13.136016171884989,{"$f":"F180*(1-Elteq!$F$8)","v":13.136016171884989}]
["REIKU-G","PAGVG-36M50",null,null,10,5.8712056563926049,{"$f":"F181*(1-Elteq!$F$8)","v":5.8712056563926049}]
["REIKU-G","PAGVG-36P29",null,null,10,5.4840931955315542,{"$f":"F182*(1-Elteq!$F$8)","v":5.4840931955315542}]
["REIKU-G","PAGVG-36P36",null,null,10,5.5615156877037641,{"$f":"F183*(1-Elteq!$F$8)","v":5.5615156877037641}]
["REIKU-G","PAGVG-36P36Z",null,null,10,13.032786182322042,{"$f":"F184*(1-Elteq!$F$8)","v":13.032786182322042}]
["REIKU-G","PAGVG-48M50",null,null,10,7.3680405050553359,{"$f":"F185*(1-Elteq!$F$8)","v":7.3680405050553359}]
["REIKU-G","PAGVG-48M63",null,null,10,7.5615967354858586,{"$f":"F186*(1-Elteq!$F$8)","v":7.5615967354858586}]
["REIKU-G","PAGVG-48M63Z",null,null,10,15.497402183137401,{"$f":"F187*(1-Elteq!$F$8)","v":15.497402183137401}]
["REIKU-G","PAGVG-48P42",null,null,10,7.6519229763534371,{"$f":"F188*(1-Elteq!$F$8)","v":7.6519229763534371}]
["REIKU-G","PAGVG-48P48",null,null,10,7.1228692798433322,{"$f":"F189*(1-Elteq!$F$8)","v":7.1228692798433322}]
["REIKU-G","PAGVG-48P48Z",null,null,10,15.032867230104134,{"$f":"F190*(1-Elteq!$F$8)","v":15.032867230104134}]
["REIKU-G","PAHDG-07",null,null,100,0.65809118346378659,{"$f":"F191*(1-Elteq!$F$8)","v":0.65809118346378659}]
["REIKU-G","PAHDG-10",null,null,100,0.67099493215915484,{"$f":"F192*(1-Elteq!$F$8)","v":0.67099493215915484}]
["REIKU-G","PAHDG-12",null,null,50,0.69680242954989124,{"$f":"F193*(1-Elteq!$F$8)","v":0.69680242954989124}]
["REIKU-G","PAHDG-14",null,null,50,0.74841742433136493,{"$f":"F194*(1-Elteq!$F$8)","v":0.74841742433136493}]
["REIKU-G","PAHDG-17",null,null,50,0.7613211730267333,{"$f":"F195*(1-Elteq!$F$8)","v":0.7613211730267333}]
["REIKU-G","PAHDG-23",null,null,50,1.3807011104044142,{"$f":"F196*(1-Elteq!$F$8)","v":1.3807011104044142}]
["REIKU-G","PAHDG-29",null,null,30,1.7420060738747289,{"$f":"F197*(1-Elteq!$F$8)","v":1.7420060738747289}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-G"},"PAHDG-36",null,null,20,2.2194447756033582,{"$f":"F198*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-G","PAHDG-48",null,null,20,2.8646322103717763,{"$f":"F199*(1-Elteq!$F$8)","v":2.8646322103717763}]
["REIKU-G","PAHOG-07",null,null,100,0.41291995825178751,{"$f":"F200*(1-Elteq!$F$8)","v":0.41291995825178751}]
["REIKU-G","PAHOG-10",null,null,100,0.42582370694715577,{"$f":"F201*(1-Elteq!$F$8)","v":0.42582370694715577}]
["REIKU-G","PAHOG-12",null,null,50,0.43872745564252419,{"$f":"F202*(1-Elteq!$F$8)","v":0.43872745564252419}]
["REIKU-G","PAHOG-14",null,null,50,0.47743870172862929,{"$f":"F203*(1-Elteq!$F$8)","v":0.47743870172862929}]
["REIKU-G","PAHOG-17",null,null,50,0.49034245042399766,{"$f":"F204*(1-Elteq!$F$8)","v":0.49034245042399766}]
["REIKU-G","PAHOG-17S",null,null,50,0.49034245042399766,{"$f":"F205*(1-Elteq!$F$8)","v":0.49034245042399766}]
["REIKU-G","PAHOG-23",null,null,50,1.0322998956294691,{"$f":"F206*(1-Elteq!$F$8)","v":1.0322998956294691}]
["REIKU-G","PAHOG-23S",null,null,50,1.0322998956294691,{"$f":"F207*(1-Elteq!$F$8)","v":1.0322998956294691}]
["REIKU-G","PAHOG-29",null,null,30,1.264567372146099,{"$f":"F208*(1-Elteq!$F$8)","v":1.264567372146099}]
["REIKU-G","PAHOG-29S",null,null,30,1.264567372146099,{"$f":"F209*(1-Elteq!$F$8)","v":1.264567372146099}]
["REIKU-G","PAHOG-36",null,null,20,1.6774873303978866,{"$f":"F210*(1-Elteq!$F$8)","v":1.6774873303978866}]
["REIKU-G","PAHOG-36S",null,null,20,1.6774873303978866,{"$f":"F211*(1-Elteq!$F$8)","v":1.6774873303978866}]
["REIKU-G","PAHOG-36V",null,null,20,1.6774873303978866,{"$f":"F212*(1-Elteq!$F$8)","v":1.6774873303978866}]
["REIKU-G","PAHOG-48",null,null,20,2.2194447756033582,{"$f":"F213*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-G","PAHOG-48S",null,null,20,2.2194447756033582,{"$f":"F214*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-G","PAHOG-48V",null,null,20,2.2194447756033582,{"$f":"F215*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-G","PAIOG-07M081",null,null,50,1.72910232517936,{"$f":"F216*(1-Elteq!$F$8)","v":1.72910232517936}]
["REIKU-G","PAIOG-07M121",null,null,50,1.72910232517936,{"$f":"F217*(1-Elteq!$F$8)","v":1.72910232517936}]
["REIKU-G","PAIOG-07M16",null,null,50,1.72910232517936,{"$f":"F218*(1-Elteq!$F$8)","v":1.72910232517936}]
["REIKU-G","PAIOG-07P07",null,null,50,1.72910232517936,{"$f":"F219*(1-Elteq!$F$8)","v":1.72910232517936}]
["REIKU-G","PAIOG-07U05",null,null,50,1.9484660530006226,{"$f":"F220*(1-Elteq!$F$8)","v":1.9484660530006226}]
["REIKU-G","PAIOG-10M121",null,null,50,1.72910232517936,{"$f":"F221*(1-Elteq!$F$8)","v":1.72910232517936}]
["REIKU-G","PAIOG-10M16",null,null,50,1.72910232517936,{"$f":"F222*(1-Elteq!$F$8)","v":1.72910232517936}]
["REIKU-G","PAIOG-10M181",null,null,50,1.72910232517936,{"$f":"F223*(1-Elteq!$F$8)","v":1.72910232517936}]
["REIKU-G","PAIOG-10P07",null,null,50,1.72910232517936,{"$f":"F224*(1-Elteq!$F$8)","v":1.72910232517936}]
["REIKU-G","PAIOG-10P09",null,null,50,1.72910232517936,{"$f":"F225*(1-Elteq!$F$8)","v":1.72910232517936}]
["REIKU-G","PAIOG-10U05",null,null,50,1.9484660530006226,{"$f":"F226*(1-Elteq!$F$8)","v":1.9484660530006226}]
["REIKU-G","PAIOG-10U07",null,null,50,1.9484660530006226,{"$f":"F227*(1-Elteq!$F$8)","v":1.9484660530006226}]
["REIKU-G","PAIOG-12M16",null,null,50,1.7678135712654652,{"$f":"F228*(1-Elteq!$F$8)","v":1.7678135712654652}]
["REIKU-G","PAIOG-12M20",null,null,50,1.7678135712654652,{"$f":"F229*(1-Elteq!$F$8)","v":1.7678135712654652}]
["REIKU-G","PAIOG-12P11",null,null,50,1.7678135712654652,{"$f":"F230*(1-Elteq!$F$8)","v":1.7678135712654652}]
["REIKU-G","PAIOG-12P13",null,null,50,1.7678135712654652,{"$f":"F231*(1-Elteq!$F$8)","v":1.7678135712654652}]
["REIKU-G","PAIOG-12U05",null,null,50,2.0129847964774643,{"$f":"F232*(1-Elteq!$F$8)","v":2.0129847964774643}]
["REIKU-G","PAIOG-12U06",null,null,50,2.0129847964774643,{"$f":"F233*(1-Elteq!$F$8)","v":2.0129847964774643}]
["REIKU-G","PAIOG-12U07",null,null,50,2.0129847964774643,{"$f":"F234*(1-Elteq!$F$8)","v":2.0129847964774643}]
["REIKU-G","PAIOG-12U09",null,null,50,2.0129847964774643,{"$f":"F235*(1-Elteq!$F$8)","v":2.0129847964774643}]
["REIKU-G","PAIOG-12U10",null,null,50,2.0129847964774643,{"$f":"F236*(1-Elteq!$F$8)","v":2.0129847964774643}]
["REIKU-G","PAIOG-17M20",null,null,50,1.8323323147423072,{"$f":"F237*(1-Elteq!$F$8)","v":1.8323323147423072}]
["REIKU-G","PAIOG-17P13",null,null,50,1.8323323147423072,{"$f":"F238*(1-Elteq!$F$8)","v":1.8323323147423072}]
["REIKU-G","PAIOG-17P16",null,null,50,1.8323323147423072,{"$f":"F239*(1-Elteq!$F$8)","v":1.8323323147423072}]
["REIKU-G","PAIOG-17U07",null,null,50,2.0645997912589382,{"$f":"F240*(1-Elteq!$F$8)","v":2.0645997912589382}]
["REIKU-G","PAIOG-17U09",null,null,50,2.0645997912589382,{"$f":"F241*(1-Elteq!$F$8)","v":2.0645997912589382}]
["REIKU-G","PAIOG-17U10",null,null,50,2.0645997912589382,{"$f":"F242*(1-Elteq!$F$8)","v":2.0645997912589382}]
["REIKU-G","PAIOG-17U11",null,null,50,2.0645997912589382,{"$f":"F243*(1-Elteq!$F$8)","v":2.0645997912589382}]
["REIKU-G","PAIOG-17U14",null,null,50,2.0645997912589382,{"$f":"F244*(1-Elteq!$F$8)","v":2.0645997912589382}]
["REIKU-G","PAIOG-17U17",null,null,50,2.0645997912589382,{"$f":"F245*(1-Elteq!$F$8)","v":2.0645997912589382}]
["REIKU-G","PAIOG-23M25",null,null,30,3.8711246086105069,{"$f":"F246*(1-Elteq!$F$8)","v":3.8711246086105069}]
["REIKU-G","PAIOG-23P21",null,null,30,3.8711246086105069,{"$f":"F247*(1-Elteq!$F$8)","v":3.8711246086105069}]
["REIKU-G","PAIOG-23U14",null,null,30,4.3614670590345064,{"$f":"F248*(1-Elteq!$F$8)","v":4.3614670590345064}]
["REIKU-G","PAIOG-23U17",null,null,30,4.3614670590345064,{"$f":"F249*(1-Elteq!$F$8)","v":4.3614670590345064}]
["REIKU-G","PAIOG-23U18",null,null,30,4.3614670590345064,{"$f":"F250*(1-Elteq!$F$8)","v":4.3614670590345064}]
["REIKU-G","PAIOG-29M32",null,null,30,6.555104337247128,{"$f":"F251*(1-Elteq!$F$8)","v":6.555104337247128}]
["REIKU-G","PAIOG-29P29",null,null,30,6.3815227258016343,{"$f":"F252*(1-Elteq!$F$8)","v":6.3815227258016343}]
["REIKU-G","PAIOG-29U24",null,null,30,6.5422005885517578,{"$f":"F253*(1-Elteq!$F$8)","v":6.5422005885517578}]
["REIKU-G","PAIOG-36M40",null,null,10,6.6196230807239651,{"$f":"F254*(1-Elteq!$F$8)","v":6.6196230807239651}]
["REIKU-G","PAIOG-36P36",null,null,10,6.6196230807239651,{"$f":"F255*(1-Elteq!$F$8)","v":6.6196230807239651}]
["REIKU-G","PAIOG-48M50",null,null,10,12.400502496248995,{"$f":"F256*(1-Elteq!$F$8)","v":12.400502496248995}]
["REIKU-G","PAIOG-48P48",null,null,10,12.400502496248995,{"$f":"F257*(1-Elteq!$F$8)","v":12.400502496248995}]
["REIKU-G","PAIRG-07M081",null,null,50,1.9226585556098852,{"$f":"F258*(1-Elteq!$F$8)","v":1.9226585556098852}]
["REIKU-G","PAIRG-07M121",null,null,50,1.9226585556098852,{"$f":"F259*(1-Elteq!$F$8)","v":1.9226585556098852}]
["REIKU-G","PAIRG-07M16",null,null,50,1.9226585556098852,{"$f":"F260*(1-Elteq!$F$8)","v":1.9226585556098852}]
["REIKU-G","PAIRG-07P07",null,null,50,1.9226585556098852,{"$f":"F261*(1-Elteq!$F$8)","v":1.9226585556098852}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-G"},"PAIRG-10M121",null,null,50,1.9355623043052534,{"$f":"F262*(1-Elteq!$F$8)","v":1.9355623043052534}]
["REIKU-G","PAIRG-10M16",null,null,50,1.9355623043052534,{"$f":"F263*(1-Elteq!$F$8)","v":1.9355623043052534}]
["REIKU-G","PAIRG-10M181",null,null,50,1.9355623043052534,{"$f":"F264*(1-Elteq!$F$8)","v":1.9355623043052534}]
["REIKU-G","PAIRG-10P07",null,null,50,1.9355623043052534,{"$f":"F265*(1-Elteq!$F$8)","v":1.9355623043052534}]
["REIKU-G","PAIRG-10P09",null,null,50,1.9355623043052534,{"$f":"F266*(1-Elteq!$F$8)","v":1.9355623043052534}]
["REIKU-G","PAIRG-12M16",null,null,50,1.987177299086728,{"$f":"F267*(1-Elteq!$F$8)","v":1.987177299086728}]
["REIKU-G","PAIRG-12M20",null,null,50,1.987177299086728,{"$f":"F268*(1-Elteq!$F$8)","v":1.987177299086728}]
["REIKU-G","PAIRG-12P11",null,null,50,1.987177299086728,{"$f":"F269*(1-Elteq!$F$8)","v":1.987177299086728}]
["REIKU-G","PAIRG-12P13",null,null,50,1.987177299086728,{"$f":"F270*(1-Elteq!$F$8)","v":1.987177299086728}]
["REIKU-G","PAIRG-17M20",null,null,50,2.0645997912589382,{"$f":"F271*(1-Elteq!$F$8)","v":2.0645997912589382}]
["REIKU-G","PAIRG-17P13",null,null,50,2.0645997912589382,{"$f":"F272*(1-Elteq!$F$8)","v":2.0645997912589382}]
["REIKU-G","PAIRG-17P16",null,null,50,2.0645997912589382,{"$f":"F273*(1-Elteq!$F$8)","v":2.0645997912589382}]
["REIKU-G","PAIRG-23M25",null,null,30,4.2840445668622964,{"$f":"F274*(1-Elteq!$F$8)","v":4.2840445668622964}]
["REIKU-G","PAIRG-23P21",null,null,30,4.2840445668622964,{"$f":"F275*(1-Elteq!$F$8)","v":4.2840445668622964}]
["REIKU-G","PAIRG-29M32",null,null,30,7.0712542850618609,{"$f":"F276*(1-Elteq!$F$8)","v":7.0712542850618609}]
["REIKU-G","PAIRG-29P29",null,null,30,7.0712542850618609,{"$f":"F277*(1-Elteq!$F$8)","v":7.0712542850618609}]
["REIKU-G","PAIRG-36M40",null,null,10,7.4067517511414405,{"$f":"F278*(1-Elteq!$F$8)","v":7.4067517511414405}]
["REIKU-G","PAIRG-36P36",null,null,10,7.4067517511414405,{"$f":"F279*(1-Elteq!$F$8)","v":7.4067517511414405}]
["REIKU-G","PAIRG-48M50",null,null,10,13.381187397096991,{"$f":"F280*(1-Elteq!$F$8)","v":13.381187397096991}]
["REIKU-G","PAIRG-48P48",null,null,10,13.381187397096991,{"$f":"F281*(1-Elteq!$F$8)","v":13.381187397096991}]
["REIKU-G","PAKOG-M12",null,null,50,0.77422492172210156,{"$f":"F282*(1-Elteq!$F$8)","v":0.77422492172210156}]
["REIKU-G","PAKOG-M16",null,null,50,1.3677973617090466,{"$f":"F283*(1-Elteq!$F$8)","v":1.3677973617090466}]
["REIKU-G","PAKOG-M20",null,null,50,1.9097548069145172,{"$f":"F284*(1-Elteq!$F$8)","v":1.9097548069145172}]
["REIKU-G","PAKOG-M25",null,null,50,2.0129847964774643,{"$f":"F285*(1-Elteq!$F$8)","v":2.0129847964774643}]
["REIKU-G","PAKOG-M32",null,null,25,3.3162634147096686,{"$f":"F286*(1-Elteq!$F$8)","v":3.3162634147096686}]
["REIKU-G","PAKOG-M40",null,null,10,11.948871291911102,{"$f":"F287*(1-Elteq!$F$8)","v":11.948871291911102}]
["REIKU-G","PAKOG-M50",null,null,5,20.000810477820959,{"$f":"F288*(1-Elteq!$F$8)","v":20.000810477820959}]
["REIKU-G","PAKOG-M63",null,null,5,22.504137724722426,{"$f":"F289*(1-Elteq!$F$8)","v":22.504137724722426}]
["REIKU-G","PAKOG-P07",null,null,50,0.63228368607304952,{"$f":"F290*(1-Elteq!$F$8)","v":0.63228368607304952}]
["REIKU-G","PAKOG-P09",null,null,50,0.64518743476841811,{"$f":"F291*(1-Elteq!$F$8)","v":0.64518743476841811}]
["REIKU-G","PAKOG-P11",null,null,50,0.7613211730267333,{"$f":"F292*(1-Elteq!$F$8)","v":0.7613211730267333}]
["REIKU-G","PAKOG-P13",null,null,50,0.86455116258968001,{"$f":"F293*(1-Elteq!$F$8)","v":0.86455116258968001}]
["REIKU-G","PAKOG-P16",null,null,50,0.9290699060665214,{"$f":"F294*(1-Elteq!$F$8)","v":0.9290699060665214}]
["REIKU-G","PAKOG-P21",null,null,50,1.3548936130136779,{"$f":"F295*(1-Elteq!$F$8)","v":1.3548936130136779}]
["REIKU-G","PAKOG-P29",null,null,25,2.6581722312458824,{"$f":"F296*(1-Elteq!$F$8)","v":2.6581722312458824}]
["REIKU-G","PAKOG-P36",null,null,10,9.6520040241355325,{"$f":"F297*(1-Elteq!$F$8)","v":9.6520040241355325}]
["REIKU-G","PAKOG-P48",null,null,5,17.781365702217595,{"$f":"F298*(1-Elteq!$F$8)","v":17.781365702217595}]
["REIKU-G","PAMCR-29",null,null,25,1.13885636337383,{"$f":"F299*(1-Elteq!$F$8)","v":1.13885636337383}]
["REIKU-G","PAMCR-36",null,null,25,1.13885636337383,{"$f":"F300*(1-Elteq!$F$8)","v":1.13885636337383}]
["REIKU-G","PAMCR-42",null,null,25,1.13885636337383,{"$f":"F301*(1-Elteq!$F$8)","v":1.13885636337383}]
["REIKU-G","PAMCR-52",null,null,25,1.13885636337383,{"$f":"F302*(1-Elteq!$F$8)","v":1.13885636337383}]
["REIKU-G","PAMCR-70",null,null,25,1.13885636337383,{"$f":"F303*(1-Elteq!$F$8)","v":1.13885636337383}]
["REIKU-G","PANOG-07M081",null,null,50,2.2581560216894632,{"$f":"F304*(1-Elteq!$F$8)","v":2.2581560216894632}]
["REIKU-G","PANOG-07M121",null,null,50,2.2581560216894632,{"$f":"F305*(1-Elteq!$F$8)","v":2.2581560216894632}]
["REIKU-G","PANOG-07M181",null,null,50,2.2581560216894632,{"$f":"F306*(1-Elteq!$F$8)","v":2.2581560216894632}]
["REIKU-G","PANOG-07M301",null,null,50,2.5678459903783031,{"$f":"F307*(1-Elteq!$F$8)","v":2.5678459903783031}]
["REIKU-G","PANOG-10M081",null,null,50,2.2581560216894632,{"$f":"F308*(1-Elteq!$F$8)","v":2.2581560216894632}]
["REIKU-G","PANOG-10M121",null,null,50,2.2581560216894632,{"$f":"F309*(1-Elteq!$F$8)","v":2.2581560216894632}]
["REIKU-G","PANOG-10M181",null,null,50,2.2581560216894632,{"$f":"F310*(1-Elteq!$F$8)","v":2.2581560216894632}]
["REIKU-G","PANOG-10M301",null,null,50,2.5678459903783031,{"$f":"F311*(1-Elteq!$F$8)","v":2.5678459903783031}]
["REIKU-G","PAREG–07G",null,null,100,0.53015727260505874,{"$f":"F312*(1-Elteq!$F$8)","v":0.53015727260505874}]
["REIKU-G","PAREG–10F",null,null,100,0.55764690896235813,{"$f":"F313*(1-Elteq!$F$8)","v":0.55764690896235813}]
["REIKU-G","PAREG–12F",null,null,50,0.69902218165704055,{"$f":"F314*(1-Elteq!$F$8)","v":0.69902218165704055}]
["REIKU-G","PAREG–14F",null,null,50,0.92286636342362072,{"$f":"F315*(1-Elteq!$F$8)","v":0.92286636342362072}]
["REIKU-G","PAREG–17F",null,null,50,0.98550346340918149,{"$f":"F316*(1-Elteq!$F$8)","v":0.98550346340918149}]
["REIKU-G","PAREG–23F",null,null,50,1.771117999591715,{"$f":"F317*(1-Elteq!$F$8)","v":1.771117999591715}]
["REIKU-G","PAREG–29F",null,null,30,2.1284832722366067,{"$f":"F318*(1-Elteq!$F$8)","v":2.1284832722366067}]
["REIKU-G","PAREG–36F",null,null,30,3.1632717265435177,{"$f":"F319*(1-Elteq!$F$8)","v":3.1632717265435177}]
["REIKU-G","PAREG-48F",null,null,30,4.4788471807857011,{"$f":"F320*(1-Elteq!$F$8)","v":4.4788471807857011}]
["REIKU-G","PAREG–52G",null,null,"10/30",6.5346792712208721,{"$f":"F321*(1-Elteq!$F$8)","v":6.5346792712208721}]
["REIKU-G","PAREG–70G",null,null,"10/30",11.742001815475005,{"$f":"F322*(1-Elteq!$F$8)","v":11.742001815475005}]
["REIKU-G","PAREG–95G",null,null,"10/30",15.943989087233621,{"$f":"F323*(1-Elteq!$F$8)","v":15.943989087233621}]
["REIKU-G","PARNG–07G",null,null,100,0.98713677519567966,{"$f":"F324*(1-Elteq!$F$8)","v":0.98713677519567966}]
["REIKU-G","PARNG–10F",null,null,100,1.0103635228473427,{"$f":"F325*(1-Elteq!$F$8)","v":1.0103635228473427}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-G"},"PARNG–12F",null,null,50,1.3355379899706257,{"$f":"F326*(1-Elteq!$F$8)","v":1.3355379899706257}]
["REIKU-G","PARNG–14F",null,null,50,1.776846195352223,{"$f":"F327*(1-Elteq!$F$8)","v":1.776846195352223}]
["REIKU-G","PARNG–17F",null,null,50,2.2413811483854844,{"$f":"F328*(1-Elteq!$F$8)","v":2.2413811483854844}]
["REIKU-G","PARNG–17G",null,null,50,2.2413811483854844,{"$f":"F329*(1-Elteq!$F$8)","v":2.2413811483854844}]
["REIKU-G","PARNG–23F",null,null,50,3.5420790168786143,{"$f":"F330*(1-Elteq!$F$8)","v":3.5420790168786143}]
["REIKU-G","PARNG–23G",null,null,50,3.5420790168786143,{"$f":"F331*(1-Elteq!$F$8)","v":3.5420790168786143}]
["REIKU-G","PARNG–29F",null,null,50,4.0646808390410332,{"$f":"F332*(1-Elteq!$F$8)","v":4.0646808390410332}]
["REIKU-G","PARNG–29G",null,null,50,4.0646808390410332,{"$f":"F333*(1-Elteq!$F$8)","v":4.0646808390410332}]
["REIKU-G","PARNG–36F",null,null,30,6.2479951182973608,{"$f":"F334*(1-Elteq!$F$8)","v":6.2479951182973608}]
["REIKU-G","PARNG–36G",null,null,30,6.2479951182973608,{"$f":"F335*(1-Elteq!$F$8)","v":6.2479951182973608}]
["REIKU-G","PARNG–48F",null,null,30,8.8029373599802963,{"$f":"F336*(1-Elteq!$F$8)","v":8.8029373599802963}]
["REIKU-G","PARNG–48G",null,null,30,8.8029373599802963,{"$f":"F337*(1-Elteq!$F$8)","v":8.8029373599802963}]
["REIKU-G","PARNG–52G",null,null,"10/30",10.03395498551844,{"$f":"F338*(1-Elteq!$F$8)","v":10.03395498551844}]
["REIKU-G","PARNG–70G",null,null,"10/30",16.363243720596618,{"$f":"F339*(1-Elteq!$F$8)","v":16.363243720596618}]
["REIKU-G","PARNG–95G",null,null,"10/30",21.949276530821589,{"$f":"F340*(1-Elteq!$F$8)","v":21.949276530821589}]
["REIKU-G","PARRG–07G",null,null,100,1.4192444824783663,{"$f":"F341*(1-Elteq!$F$8)","v":1.4192444824783663}]
["REIKU-G","PARRG–10F",null,null,100,1.4576024414642688,{"$f":"F342*(1-Elteq!$F$8)","v":1.4576024414642688}]
["REIKU-G","PARRG–12F",null,null,50,2.0073998535955275,{"$f":"F343*(1-Elteq!$F$8)","v":2.0073998535955275}]
["REIKU-G","PARRG–17F",null,null,50,3.119780664186679,{"$f":"F344*(1-Elteq!$F$8)","v":3.119780664186679}]
["REIKU-G","PARRG–23F",null,null,50,4.9226047365240655,{"$f":"F345*(1-Elteq!$F$8)","v":4.9226047365240655}]
["REIKU-G","PARRG–23G",null,null,50,4.9226047365240655,{"$f":"F346*(1-Elteq!$F$8)","v":4.9226047365240655}]
["REIKU-G","PARRG–29F",null,null,50,6.239561328373358,{"$f":"F347*(1-Elteq!$F$8)","v":6.239561328373358}]
["REIKU-G","PARRG–29G",null,null,50,6.239561328373358,{"$f":"F348*(1-Elteq!$F$8)","v":6.239561328373358}]
["REIKU-G","PARRG-36F",null,null,30,8.8479321706876117,{"$f":"F349*(1-Elteq!$F$8)","v":8.8479321706876117}]
["REIKU-G","PARRG–36G",null,null,30,8.8479025394146813,{"$f":"F350*(1-Elteq!$F$8)","v":8.8479025394146813}]
["REIKU-G","PARRB-48F",null,null,30,12.798781978867757,{"$f":"F351*(1-Elteq!$F$8)","v":12.798781978867757}]
["REIKU-G","PARRG–48G",null,null,30,12.798772314962568,{"$f":"F352*(1-Elteq!$F$8)","v":12.798772314962568}]
["REIKU-G","PARRG–52G",null,null,30,18.565252149176473,{"$f":"F353*(1-Elteq!$F$8)","v":18.565252149176473}]
["REIKU-G","PARRG–70G",null,null,"10/30",30.238857667219246,{"$f":"F354*(1-Elteq!$F$8)","v":30.238857667219246}]
["REIKU-G","PARRG–95G",null,null,"10/30",35.020816554128345,{"$f":"F355*(1-Elteq!$F$8)","v":35.020816554128345}]
["REIKU-G","PARVG–07G",null,null,100,1.4400583544031094,{"$f":"F356*(1-Elteq!$F$8)","v":1.4400583544031094}]
["REIKU-G","PARVG–10F",null,null,100,1.4516717282289404,{"$f":"F357*(1-Elteq!$F$8)","v":1.4516717282289404}]
["REIKU-G","PARVG–12F",null,null,50,1.9162066812622018,{"$f":"F358*(1-Elteq!$F$8)","v":1.9162066812622018}]
["REIKU-G","PARVG–17F",null,null,50,3.658212755136931,{"$f":"F359*(1-Elteq!$F$8)","v":3.658212755136931}]
["REIKU-G","PARVG–17G",null,null,50,3.658212755136931,{"$f":"F360*(1-Elteq!$F$8)","v":3.658212755136931}]
["REIKU-G","PARVG–23F",null,null,50,5.5163525672699754,{"$f":"F361*(1-Elteq!$F$8)","v":5.5163525672699754}]
["REIKU-G","PARVG–23G",null,null,50,5.5163525672699754,{"$f":"F362*(1-Elteq!$F$8)","v":5.5163525672699754}]
["REIKU-G","PARVG–29G",null,null,50,6.4338090995106674,{"$f":"F363*(1-Elteq!$F$8)","v":6.4338090995106674}]
["REIKU-G","PARVG–36G",null,null,30,10.289449209686733,{"$f":"F364*(1-Elteq!$F$8)","v":10.289449209686733}]
["REIKU-G","PARVG–48G",null,null,30,12.286949507729748,{"$f":"F365*(1-Elteq!$F$8)","v":12.286949507729748}]
["REIKU-G","PARVG–52G",null,null,"10/30",17.780075327348069,{"$f":"F366*(1-Elteq!$F$8)","v":17.780075327348069}]
["REIKU-G","PARVG–70G",null,null,"10/30",28.998594443101318,{"$f":"F367*(1-Elteq!$F$8)","v":28.998594443101318}]
["REIKU-G","PARVG–95G",null,null,"10/30",34.665920870107094,{"$f":"F368*(1-Elteq!$F$8)","v":34.665920870107094}]
["REIKU-G","PASOG-07M12",null,null,50,2.4259047547292516,{"$f":"F369*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-G","PASOG-07M12",null,null,50,2.4259047547292516,{"$f":"F370*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-G","PASOG-07M16",null,null,50,2.4259047547292516,{"$f":"F371*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-G","PASOG-07M16",null,null,50,2.4259047547292516,{"$f":"F372*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-G","PASOG-07M20",null,null,50,2.4259047547292516,{"$f":"F373*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-G","PASOG-07M20",null,null,50,2.4259047547292516,{"$f":"F374*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-G","PASOG-07P07",null,null,50,2.4259047547292516,{"$f":"F375*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-G","PASOG-07P09",null,null,50,2.4259047547292516,{"$f":"F376*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-G","PASOG-07P11",null,null,50,2.4259047547292516,{"$f":"F377*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-G","PASOG-07P13",null,null,50,2.4259047547292516,{"$f":"F378*(1-Elteq!$F$8)","v":2.4259047547292516}]
["REIKU-G","PASOG-17M25",null,null,50,3.1743221790606166,{"$f":"F379*(1-Elteq!$F$8)","v":3.1743221790606166}]
["REIKU-G","PASOG-17P16",null,null,50,3.1743221790606166,{"$f":"F380*(1-Elteq!$F$8)","v":3.1743221790606166}]
["REIKU-G","PASOG-23M32",null,null,30,4.6969645251140832,{"$f":"F381*(1-Elteq!$F$8)","v":4.6969645251140832}]
["REIKU-G","PASOG-23P21",null,null,30,4.6969645251140832,{"$f":"F382*(1-Elteq!$F$8)","v":4.6969645251140832}]
["REIKU-G","PASOG-52",null,null,10,24.804487948827429,{"$f":"F383*(1-Elteq!$F$8)","v":24.804487948827429}]
["REIKU-G","PASOG-70",null,null,10,33.652976597520684,{"$f":"F384*(1-Elteq!$F$8)","v":33.652976597520684}]
["REIKU-G","PASOG-95",null,null,10,42.879156914709057,{"$f":"F385*(1-Elteq!$F$8)","v":42.879156914709057}]
["REIKU-G","PASVG-07M12",null,null,50,2.7614022208088285,{"$f":"F386*(1-Elteq!$F$8)","v":2.7614022208088285}]
["REIKU-G","PASVG-07M12",null,null,50,2.7614022208088285,{"$f":"F387*(1-Elteq!$F$8)","v":2.7614022208088285}]
["REIKU-G","PASVG-07M16",null,null,50,2.7743059695041974,{"$f":"F388*(1-Elteq!$F$8)","v":2.7743059695041974}]
["REIKU-G","PASVG-07M16",null,null,50,2.7743059695041974,{"$f":"F389*(1-Elteq!$F$8)","v":2.7743059695041974}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-G"},"PASVG-07M20",null,null,50,2.8130172155903033,{"$f":"F390*(1-Elteq!$F$8)","v":2.8130172155903033}]
["REIKU-G","PASVG-07M20",null,null,50,2.8130172155903033,{"$f":"F391*(1-Elteq!$F$8)","v":2.8130172155903033}]
["REIKU-G","PASVG-07P07",null,null,50,2.7614022208088285,{"$f":"F392*(1-Elteq!$F$8)","v":2.7614022208088285}]
["REIKU-G","PASVG-07P09",null,null,50,2.7614022208088285,{"$f":"F393*(1-Elteq!$F$8)","v":2.7614022208088285}]
["REIKU-G","PASVG-07P11",null,null,50,2.7743059695041974,{"$f":"F394*(1-Elteq!$F$8)","v":2.7743059695041974}]
["REIKU-G","PASVG-07P13",null,null,50,2.787209718199565,{"$f":"F395*(1-Elteq!$F$8)","v":2.787209718199565}]
["REIKU-G","PASVG-17M25",null,null,50,3.638857132093877,{"$f":"F396*(1-Elteq!$F$8)","v":3.638857132093877}]
["REIKU-G","PASVG-17P16",null,null,50,3.6001458860077729,{"$f":"F397*(1-Elteq!$F$8)","v":3.6001458860077729}]
["REIKU-G","PASVG-23M32",null,null,30,5.4324782007500803,{"$f":"F398*(1-Elteq!$F$8)","v":5.4324782007500803}]
["REIKU-G","PASVG-23P21",null,null,30,5.3421519598825027,{"$f":"F399*(1-Elteq!$F$8)","v":5.3421519598825027}]
["REIKU-G","PAVSG",null,null,100,7.7422492172210172E-2,{"$f":"F400*(1-Elteq!$F$8)","v":7.7422492172210172E-2}]
["REIKU-G","PAWOG-07P07",null,null,50,2.2065410269079901,{"$f":"F401*(1-Elteq!$F$8)","v":2.2065410269079901}]
["REIKU-G","PAWOG-10M16",null,null,50,2.2194447756033582,{"$f":"F402*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-G","PAWOG-10M20",null,null,50,2.2194447756033582,{"$f":"F403*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-G","PAWOG-10P07",null,null,50,2.2065410269079901,{"$f":"F404*(1-Elteq!$F$8)","v":2.2065410269079901}]
["REIKU-G","PAWOG-10P09",null,null,50,2.2194447756033582,{"$f":"F405*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-G","PAWOG-10P11",null,null,50,2.2194447756033582,{"$f":"F406*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-G","PAWOG-12M16",null,null,50,2.2194447756033582,{"$f":"F407*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-G","PAWOG-12M20",null,null,50,2.2194447756033582,{"$f":"F408*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-G","PAWOG-12P09",null,null,50,2.2194447756033582,{"$f":"F409*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-G","PAWOG-12P11",null,null,50,2.2194447756033582,{"$f":"F410*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-G","PAWOG-12P13",null,null,50,2.2194447756033582,{"$f":"F411*(1-Elteq!$F$8)","v":2.2194447756033582}]
["REIKU-G","PAWOG-17M20",null,null,50,1.8820583177479586,{"$f":"F412*(1-Elteq!$F$8)","v":1.8820583177479586}]
["REIKU-G","PAWOG-17M25",null,null,50,2.2323548267581161,{"$f":"F413*(1-Elteq!$F$8)","v":2.2323548267581161}]
["REIKU-G","PAWOG-17P13",null,null,50,2.2323485242987262,{"$f":"F414*(1-Elteq!$F$8)","v":2.2323485242987262}]
["REIKU-G","PAWOG-17P16",null,null,50,2.2323485242987262,{"$f":"F415*(1-Elteq!$F$8)","v":2.2323485242987262}]
["REIKU-G","PAWOG-23M25",null,null,30,3.7162796242660856,{"$f":"F416*(1-Elteq!$F$8)","v":3.7162796242660856}]
["REIKU-G","PAWOG-23P21",null,null,30,3.7162796242660856,{"$f":"F417*(1-Elteq!$F$8)","v":3.7162796242660856}]
["REIKU-G","PAWOG-29M32",null,null,30,5.3292482111871333,{"$f":"F418*(1-Elteq!$F$8)","v":5.3292482111871333}]
["REIKU-G","PAWOG-29P29",null,null,30,5.3292482111871333,{"$f":"F419*(1-Elteq!$F$8)","v":5.3292482111871333}]
["REIKU-G","PAWOG-36M40",null,null,10,8.8003566102412201,{"$f":"F420*(1-Elteq!$F$8)","v":8.8003566102412201}]
["REIKU-G","PAWOG-36P36",null,null,10,8.8003566102412201,{"$f":"F421*(1-Elteq!$F$8)","v":8.8003566102412201}]
["REIKU-G","PAWOG-48M50",null,null,10,9.8326565058706912,{"$f":"F422*(1-Elteq!$F$8)","v":9.8326565058706912}]
["REIKU-G","PAWOG-48P48",null,null,10,9.8326565058706912,{"$f":"F423*(1-Elteq!$F$8)","v":9.8326565058706912}]
["REIKU-G","PAWOG-52",null,null,10,15.75489966000448,{"$f":"F424*(1-Elteq!$F$8)","v":15.75489966000448}]
["REIKU-G","PAWOG-70",null,null,10,22.258966499510418,{"$f":"F425*(1-Elteq!$F$8)","v":22.258966499510418}]
["REIKU-G","PAWOG-95",null,null,10,28.994723318492724,{"$f":"F426*(1-Elteq!$F$8)","v":28.994723318492724}]
["REIKU-G","PAWVG-07P07",null,null,50,2.5549422416829355,{"$f":"F427*(1-Elteq!$F$8)","v":2.5549422416829355}]
["REIKU-G","PAWVG-10M16",null,null,50,2.5936534877690405,{"$f":"F428*(1-Elteq!$F$8)","v":2.5936534877690405}]
["REIKU-G","PAWVG-10M20",null,null,50,2.6323647338551464,{"$f":"F429*(1-Elteq!$F$8)","v":2.6323647338551464}]
["REIKU-G","PAWVG-10P07",null,null,50,2.5678459903783031,{"$f":"F430*(1-Elteq!$F$8)","v":2.5678459903783031}]
["REIKU-G","PAWVG-10P09",null,null,50,2.5807497390736724,{"$f":"F431*(1-Elteq!$F$8)","v":2.5807497390736724}]
["REIKU-G","PAWVG-10P11",null,null,50,2.5936534877690405,{"$f":"F432*(1-Elteq!$F$8)","v":2.5936534877690405}]
["REIKU-G","PAWVG-10P11K",null,null,50,2.5936534877690405,{"$f":"F433*(1-Elteq!$F$8)","v":2.5936534877690405}]
["REIKU-G","PAWVG-10P13",null,null,50,2.6065572364644094,{"$f":"F434*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-G","PAWVG-12M16",null,null,50,2.6065572364644094,{"$f":"F435*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-G","PAWVG-12M20",null,null,50,2.6452684825505144,{"$f":"F436*(1-Elteq!$F$8)","v":2.6452684825505144}]
["REIKU-G","PAWVG-12P09",null,null,50,2.5936534877690405,{"$f":"F437*(1-Elteq!$F$8)","v":2.5936534877690405}]
["REIKU-G","PAWVG-12P11",null,null,50,2.6065572364644094,{"$f":"F438*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-G","PAWVG-12P13",null,null,50,2.6194609851597779,{"$f":"F439*(1-Elteq!$F$8)","v":2.6194609851597779}]
["REIKU-G","PAWVG-17M20",null,null,50,2.6710759799412513,{"$f":"F440*(1-Elteq!$F$8)","v":2.6710759799412513}]
["REIKU-G","PAWVG-17P13",null,null,50,2.6452684825505144,{"$f":"F441*(1-Elteq!$F$8)","v":2.6452684825505144}]
["REIKU-G","PAWVG-17P16",null,null,50,2.6581722312458824,{"$f":"F442*(1-Elteq!$F$8)","v":2.6581722312458824}]
["REIKU-G","PAWVG-23M25",null,null,30,4.3614670590345064,{"$f":"F443*(1-Elteq!$F$8)","v":4.3614670590345064}]
["REIKU-G","PAWVG-23P21",null,null,30,4.3614670590345064,{"$f":"F444*(1-Elteq!$F$8)","v":4.3614670590345064}]
["REIKU-G","PAWVG-29M32",null,null,30,6.1808956250814449,{"$f":"F445*(1-Elteq!$F$8)","v":6.1808956250814449}]
["REIKU-G","PAWVG-29P29",null,null,30,6.1808956250814449,{"$f":"F446*(1-Elteq!$F$8)","v":6.1808956250814449}]
["REIKU-G","PAWVG-36M40",null,null,10,10.090731479778055,{"$f":"F447*(1-Elteq!$F$8)","v":10.090731479778055}]
["REIKU-G","PAWVG-36P36",null,null,10,9.9875014902151147,{"$f":"F448*(1-Elteq!$F$8)","v":9.9875014902151147}]
["REIKU-G","PAWVG-48M50",null,null,10,11.523047584963946,{"$f":"F449*(1-Elteq!$F$8)","v":11.523047584963946}]
["REIKU-G","PAWVG-48P48",null,null,10,11.277876359751948,{"$f":"F450*(1-Elteq!$F$8)","v":11.277876359751948}]
["REIKU-G","PEREG-10F",null,null,100,0.67357568189822858,{"$f":"F451*(1-Elteq!$F$8)","v":0.67357568189822858}]
["REIKU-G","PEREG-12F",null,null,50,0.70841580337572319,{"$f":"F452*(1-Elteq!$F$8)","v":0.70841580337572319}]
["REIKU-G","PEREG-17F",null,null,50,0.9290699060665214,{"$f":"F453*(1-Elteq!$F$8)","v":0.9290699060665214}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-G"},"PEREG-23F",null,null,50,1.1845641302348153,{"$f":"F454*(1-Elteq!$F$8)","v":1.1845641302348153}]
["REIKU-G","PEREG-29F",null,null,50,1.4168316067514464,{"$f":"F455*(1-Elteq!$F$8)","v":1.4168316067514464}]
["REIKU-G","PEREG-36M",null,null,30,2.2762212698629791,{"$f":"F456*(1-Elteq!$F$8)","v":2.2762212698629791}]
["REIKU-G","PEREG-48M",null,null,30,2.9033434564578808,{"$f":"F457*(1-Elteq!$F$8)","v":2.9033434564578808}]
["REIKU-G","PKNOG-07M081",null,null,50,2.2581560216894632,{"$f":"F458*(1-Elteq!$F$8)","v":2.2581560216894632}]
["REIKU-G","PKNOG-07M121",null,null,50,2.2581560216894632,{"$f":"F459*(1-Elteq!$F$8)","v":2.2581560216894632}]
["REIKU-G","PMAOG-07P07",null,null,30,3.4840121477494579,{"$f":"F460*(1-Elteq!$F$8)","v":3.4840121477494579}]
["REIKU-G","PMAOG-10P09",null,null,30,3.4840121477494579,{"$f":"F461*(1-Elteq!$F$8)","v":3.4840121477494579}]
["REIKU-G","PMAOG-12P11",null,null,30,3.8582208599151402,{"$f":"F462*(1-Elteq!$F$8)","v":3.8582208599151402}]
["REIKU-G","PMAOG-17P16",null,null,30,4.3356595616437694,{"$f":"F463*(1-Elteq!$F$8)","v":4.3356595616437694}]
["REIKU-G","PMAOG-23P21",null,null,30,6.684141824200811,{"$f":"F464*(1-Elteq!$F$8)","v":6.684141824200811}]
["REIKU-G","PMAOG-29P29",null,null,20,8.2454954163403791,{"$f":"F465*(1-Elteq!$F$8)","v":8.2454954163403791}]
["REIKU-G","PMAVG-07P07",null,null,30,3.8195096138290343,{"$f":"F466*(1-Elteq!$F$8)","v":3.8195096138290343}]
["REIKU-G","PMAVG-10P09",null,null,30,3.8324133625244037,{"$f":"F467*(1-Elteq!$F$8)","v":3.8324133625244037}]
["REIKU-G","PMAVG-12P11",null,null,30,4.2453333207761919,{"$f":"F468*(1-Elteq!$F$8)","v":4.2453333207761919}]
["REIKU-G","PMAVG-17P16",null,null,30,4.7614832685909265,{"$f":"F469*(1-Elteq!$F$8)","v":4.7614832685909265}]
["REIKU-G","PMAVG-23P21",null,null,30,7.3293292589692287,{"$f":"F470*(1-Elteq!$F$8)","v":7.3293292589692287}]
["REIKU-G","PMAVG-29P29",null,null,20,9.084239081539323,{"$f":"F471*(1-Elteq!$F$8)","v":9.084239081539323}]
["REIKU-G","PMGOG-07M12Z",null,null,30,6.0389543894323916,{"$f":"F472*(1-Elteq!$F$8)","v":6.0389543894323916}]
["REIKU-G","PMGOG-07P07",null,null,50,2.6323647338551464,{"$f":"F473*(1-Elteq!$F$8)","v":2.6323647338551464}]
["REIKU-G","PMGOG-07P07Z",null,null,30,6.0389543894323916,{"$f":"F474*(1-Elteq!$F$8)","v":6.0389543894323916}]
["REIKU-G","PMGOG-10M16",null,null,30,2.6323647338551464,{"$f":"F475*(1-Elteq!$F$8)","v":2.6323647338551464}]
["REIKU-G","PMGOG-10M16Z",null,null,30,6.0389543894323916,{"$f":"F476*(1-Elteq!$F$8)","v":6.0389543894323916}]
["REIKU-G","PMGOG-10M20",null,null,30,2.6323647338551464,{"$f":"F477*(1-Elteq!$F$8)","v":2.6323647338551464}]
["REIKU-G","PMGOG-10P09",null,null,30,2.6323647338551464,{"$f":"F478*(1-Elteq!$F$8)","v":2.6323647338551464}]
["REIKU-G","PMGOG-10P09Z",null,null,30,6.0389543894323916,{"$f":"F479*(1-Elteq!$F$8)","v":6.0389543894323916}]
["REIKU-G","PMGOG-12M16",null,null,30,3.1227071842791427,{"$f":"F480*(1-Elteq!$F$8)","v":3.1227071842791427}]
["REIKU-G","PMGOG-12M16Z",null,null,30,6.6196230807239651,{"$f":"F481*(1-Elteq!$F$8)","v":6.6196230807239651}]
["REIKU-G","PMGOG-12M20",null,null,30,3.1227071842791427,{"$f":"F482*(1-Elteq!$F$8)","v":3.1227071842791427}]
["REIKU-G","PMGOG-12M20Z",null,null,30,7.4454629972275459,{"$f":"F483*(1-Elteq!$F$8)","v":7.4454629972275459}]
["REIKU-G","PMGOG-12P11",null,null,30,3.1227071842791427,{"$f":"F484*(1-Elteq!$F$8)","v":3.1227071842791427}]
["REIKU-G","PMGOG-12P11Z",null,null,30,6.6196230807239651,{"$f":"F485*(1-Elteq!$F$8)","v":6.6196230807239651}]
["REIKU-G","PMGOG-12P13Z",null,null,30,7.4454629972275459,{"$f":"F486*(1-Elteq!$F$8)","v":7.4454629972275459}]
["REIKU-G","PMGOG-17M20",null,null,30,3.7937021164382991,{"$f":"F487*(1-Elteq!$F$8)","v":3.7937021164382991}]
["REIKU-G","PMGOG-17M20Z",null,null,30,14.245738559686664,{"$f":"F488*(1-Elteq!$F$8)","v":14.245738559686664}]
["REIKU-G","PMGOG-17M25",null,null,30,3.7937021164382991,{"$f":"F489*(1-Elteq!$F$8)","v":3.7937021164382991}]
["REIKU-G","PMGOG-17P13",null,null,30,3.7549908703521941,{"$f":"F490*(1-Elteq!$F$8)","v":3.7549908703521941}]
["REIKU-G","PMGOG-17P16",null,null,30,3.7937021164382991,{"$f":"F491*(1-Elteq!$F$8)","v":3.7937021164382991}]
["REIKU-G","PMGOG-17P16Z",null,null,30,14.245738559686664,{"$f":"F492*(1-Elteq!$F$8)","v":14.245738559686664}]
["REIKU-G","PMGOG-23M25",null,null,30,6.5163930911610208,{"$f":"F493*(1-Elteq!$F$8)","v":6.5163930911610208}]
["REIKU-G","PMGOG-23M25Z",null,null,30,17.058755775276968,{"$f":"F494*(1-Elteq!$F$8)","v":17.058755775276968}]
["REIKU-G","PMGOG-23M32",null,null,30,6.5163930911610208,{"$f":"F495*(1-Elteq!$F$8)","v":6.5163930911610208}]
["REIKU-G","PMGOG-23P21",null,null,30,6.5163930911610208,{"$f":"F496*(1-Elteq!$F$8)","v":6.5163930911610208}]
["REIKU-G","PMGOG-23P21Z",null,null,30,17.058755775276968,{"$f":"F497*(1-Elteq!$F$8)","v":17.058755775276968}]
["REIKU-G","PMGOG-29M32",null,null,20,7.8454792067839625,{"$f":"F498*(1-Elteq!$F$8)","v":7.8454792067839625}]
["REIKU-G","PMGOG-29M32Z",null,null,20,22.310581494291895,{"$f":"F499*(1-Elteq!$F$8)","v":22.310581494291895}]
["REIKU-G","PMGOG-29M40",null,null,20,7.8454792067839625,{"$f":"F500*(1-Elteq!$F$8)","v":7.8454792067839625}]
["REIKU-G","PMGOG-29P29",null,null,20,7.8454792067839625,{"$f":"F501*(1-Elteq!$F$8)","v":7.8454792067839625}]
["REIKU-G","PMGOG-29P29Z",null,null,20,22.310581494291895,{"$f":"F502*(1-Elteq!$F$8)","v":22.310581494291895}]
["REIKU-G","PMGOG-36M40Z",null,null,10,29.678621999347232,{"$f":"F503*(1-Elteq!$F$8)","v":29.678621999347232}]
["REIKU-G","PMGOG-36M50",null,null,10,12.542443731898043,{"$f":"F504*(1-Elteq!$F$8)","v":12.542443731898043}]
["REIKU-G","PMGOG-36P36",null,null,10,12.542443731898043,{"$f":"F505*(1-Elteq!$F$8)","v":12.542443731898043}]
["REIKU-G","PMGOG-36P36Z",null,null,10,29.678621999347232,{"$f":"F506*(1-Elteq!$F$8)","v":29.678621999347232}]
["REIKU-G","PMGOG-48M63",null,null,10,15.265134706620771,{"$f":"F507*(1-Elteq!$F$8)","v":15.265134706620771}]
["REIKU-G","PMGOG-48M63Z",null,null,10,43.627574339040414,{"$f":"F508*(1-Elteq!$F$8)","v":43.627574339040414}]
["REIKU-G","PMGOG-48P48",null,null,10,15.265134706620771,{"$f":"F509*(1-Elteq!$F$8)","v":15.265134706620771}]
["REIKU-G","PMGOG-48P48Z",null,null,10,43.627574339040414,{"$f":"F510*(1-Elteq!$F$8)","v":43.627574339040414}]
["REIKU-G","PMGVG-07M12Z",null,null,30,6.3873556042073378,{"$f":"F511*(1-Elteq!$F$8)","v":6.3873556042073378}]
["REIKU-G","PMGVG-07P07",null,null,50,2.9807659486300917,{"$f":"F512*(1-Elteq!$F$8)","v":2.9807659486300917}]
["REIKU-G","PMGVG-07P07Z",null,null,30,6.3873556042073378,{"$f":"F513*(1-Elteq!$F$8)","v":6.3873556042073378}]
["REIKU-G","PMGVG-10M16",null,null,30,3.0065734460208282,{"$f":"F514*(1-Elteq!$F$8)","v":3.0065734460208282}]
["REIKU-G","PMGVG-10M16Z",null,null,30,6.4131631015980748,{"$f":"F515*(1-Elteq!$F$8)","v":6.4131631015980748}]
["REIKU-G","PMGVG-10M20",null,null,30,3.0452846921069332,{"$f":"F516*(1-Elteq!$F$8)","v":3.0452846921069332}]
["REIKU-G","PMGVG-10P09",null,null,30,3.0065734460208282,{"$f":"F517*(1-Elteq!$F$8)","v":3.0065734460208282}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-G"},"PMGVG-10P09Z",null,null,30,6.4002593529027063,{"$f":"F518*(1-Elteq!$F$8)","v":6.4002593529027063}]
["REIKU-G","PMGVG-12M16",null,null,30,3.5098196451401935,{"$f":"F519*(1-Elteq!$F$8)","v":3.5098196451401935}]
["REIKU-G","PMGVG-12M16Z",null,null,30,6.9938317928896518,{"$f":"F520*(1-Elteq!$F$8)","v":6.9938317928896518}]
["REIKU-G","PMGVG-12M20",null,null,30,3.5485308912262981,{"$f":"F521*(1-Elteq!$F$8)","v":3.5485308912262981}]
["REIKU-G","PMGVG-12M20Z",null,null,30,7.8712867041746994,{"$f":"F522*(1-Elteq!$F$8)","v":7.8712867041746994}]
["REIKU-G","PMGVG-12P11",null,null,30,3.5227233938355633,{"$f":"F523*(1-Elteq!$F$8)","v":3.5227233938355633}]
["REIKU-G","PMGVG-12P11Z",null,null,30,6.9938317928896518,{"$f":"F524*(1-Elteq!$F$8)","v":6.9938317928896518}]
["REIKU-G","PMGVG-12P13Z",null,null,30,7.8454792067839625,{"$f":"F525*(1-Elteq!$F$8)","v":7.8454792067839625}]
["REIKU-G","PMGVG-17M20",null,null,30,4.2324295720808225,{"$f":"F526*(1-Elteq!$F$8)","v":4.2324295720808225}]
["REIKU-G","PMGVG-17M20Z",null,null,30,14.684466015329193,{"$f":"F527*(1-Elteq!$F$8)","v":14.684466015329193}]
["REIKU-G","PMGVG-17M25",null,null,30,4.2582370694715594,{"$f":"F528*(1-Elteq!$F$8)","v":4.2582370694715594}]
["REIKU-G","PMGVG-17P13",null,null,30,4.1808145772993504,{"$f":"F529*(1-Elteq!$F$8)","v":4.1808145772993504}]
["REIKU-G","PMGVG-17P16",null,null,30,4.2324295720808225,{"$f":"F530*(1-Elteq!$F$8)","v":4.2324295720808225}]
["REIKU-G","PMGVG-17P16Z",null,null,30,14.671562266633828,{"$f":"F531*(1-Elteq!$F$8)","v":14.671562266633828}]
["REIKU-G","PMGVG-23M25",null,null,30,7.1744842746248088,{"$f":"F532*(1-Elteq!$F$8)","v":7.1744842746248088}]
["REIKU-G","PMGVG-23M25Z",null,null,30,17.703943210045388,{"$f":"F533*(1-Elteq!$F$8)","v":17.703943210045388}]
["REIKU-G","PMGVG-23M32",null,null,30,7.2648105154923881,{"$f":"F534*(1-Elteq!$F$8)","v":7.2648105154923881}]
["REIKU-G","PMGVG-23P21",null,null,30,7.2002917720155457,{"$f":"F535*(1-Elteq!$F$8)","v":7.2002917720155457}]
["REIKU-G","PMGVG-23P21Z",null,null,30,17.703943210045388,{"$f":"F536*(1-Elteq!$F$8)","v":17.703943210045388}]
["REIKU-G","PMGVG-29M32",null,null,20,8.6842228719829055,{"$f":"F537*(1-Elteq!$F$8)","v":8.6842228719829055}]
["REIKU-G","PMGVG-29M32Z",null,null,20,23.162228908186215,{"$f":"F538*(1-Elteq!$F$8)","v":23.162228908186215}]
["REIKU-G","PMGVG-29M40",null,null,20,8.8648753537180642,{"$f":"F539*(1-Elteq!$F$8)","v":8.8648753537180642}]
["REIKU-G","PMGVG-29P29",null,null,20,8.6971266206782758,{"$f":"F540*(1-Elteq!$F$8)","v":8.6971266206782758}]
["REIKU-G","PMGVG-29P29Z",null,null,20,23.162228908186215,{"$f":"F541*(1-Elteq!$F$8)","v":23.162228908186215}]
["REIKU-G","PMGVG-36M40Z",null,null,10,30.981900617579424,{"$f":"F542*(1-Elteq!$F$8)","v":30.981900617579424}]
["REIKU-G","PMGVG-36M50",null,null,10,14.052182329256139,{"$f":"F543*(1-Elteq!$F$8)","v":14.052182329256139}]
["REIKU-G","PMGVG-36P36",null,null,10,13.729588611871932,{"$f":"F544*(1-Elteq!$F$8)","v":13.729588611871932}]
["REIKU-G","PMGVG-36P36Z",null,null,10,30.865766879321122,{"$f":"F545*(1-Elteq!$F$8)","v":30.865766879321122}]
["REIKU-G","PMGVG-48M63",null,null,10,17.17488951353528,{"$f":"F546*(1-Elteq!$F$8)","v":17.17488951353528}]
["REIKU-G","PMGVG-48M63Z",null,null,10,45.550232894650328,{"$f":"F547*(1-Elteq!$F$8)","v":45.550232894650328}]
["REIKU-G","PMGVG-48P48",null,null,10,16.723258309197401,{"$f":"F548*(1-Elteq!$F$8)","v":16.723258309197401}]
["REIKU-G","PMGVG-48P48Z",null,null,10,45.085697941617042,{"$f":"F549*(1-Elteq!$F$8)","v":45.085697941617042}]
["REIKU-G","PMSOG-07P07",null,null,30,3.6646646294846144,{"$f":"F550*(1-Elteq!$F$8)","v":3.6646646294846144}]
["REIKU-G","PMSVG-07P07",null,null,30,4.0130658442595601,{"$f":"F551*(1-Elteq!$F$8)","v":4.0130658442595601}]
["REIKU-G","PMWOG-10P09",null,null,30,3.6646646294846144,{"$f":"F552*(1-Elteq!$F$8)","v":3.6646646294846144}]
["REIKU-G","PMWOG-12M16",null,null,30,3.7162796242660856,{"$f":"F553*(1-Elteq!$F$8)","v":3.7162796242660856}]
["REIKU-G","PMWOG-12P11",null,null,30,3.7162796242660856,{"$f":"F554*(1-Elteq!$F$8)","v":3.7162796242660856}]
["REIKU-G","PMWOG-17M20",null,null,30,4.1679108286039801,{"$f":"F555*(1-Elteq!$F$8)","v":4.1679108286039801}]
["REIKU-G","PMWOG-17P13",null,null,30,4.090488336431771,{"$f":"F556*(1-Elteq!$F$8)","v":4.090488336431771}]
["REIKU-G","PMWOG-17P16",null,null,30,4.1679108286039801,{"$f":"F557*(1-Elteq!$F$8)","v":4.1679108286039801}]
["REIKU-G","PMWOG-23M25",null,null,30,6.4131631015980748,{"$f":"F558*(1-Elteq!$F$8)","v":6.4131631015980748}]
["REIKU-G","PMWOG-23P21",null,null,30,7.1873880233201763,{"$f":"F559*(1-Elteq!$F$8)","v":7.1873880233201763}]
["REIKU-G","PMWOG-29M32",null,null,20,7.9099979502608058,{"$f":"F560*(1-Elteq!$F$8)","v":7.9099979502608058}]
["REIKU-G","PMWOG-29P29",null,null,20,7.9099979502608058,{"$f":"F561*(1-Elteq!$F$8)","v":7.9099979502608058}]
["REIKU-G","PMWOG-36M40",null,null,10,13.277957407534041,{"$f":"F562*(1-Elteq!$F$8)","v":13.277957407534041}]
["REIKU-G","PMWOG-36P36",null,null,10,13.277957407534041,{"$f":"F563*(1-Elteq!$F$8)","v":13.277957407534041}]
["REIKU-G","PMWOG-48M50",null,null,10,19.807254247390436,{"$f":"F564*(1-Elteq!$F$8)","v":19.807254247390436}]
["REIKU-G","PMWOG-48P48",null,null,10,19.807254247390436,{"$f":"F565*(1-Elteq!$F$8)","v":19.807254247390436}]
["REIKU-G","PMWVG-10P09",null,null,30,4.0259695929549286,{"$f":"F566*(1-Elteq!$F$8)","v":4.0259695929549286}]
["REIKU-G","PMWVG-12M16",null,null,30,4.1033920851271395,{"$f":"F567*(1-Elteq!$F$8)","v":4.1033920851271395}]
["REIKU-G","PMWVG-12P11",null,null,30,4.1033920851271395,{"$f":"F568*(1-Elteq!$F$8)","v":4.1033920851271395}]
["REIKU-G","PMWVG-17M20",null,null,30,4.6066382842465039,{"$f":"F569*(1-Elteq!$F$8)","v":4.6066382842465039}]
["REIKU-G","PMWVG-17P13",null,null,30,4.5034082946835579,{"$f":"F570*(1-Elteq!$F$8)","v":4.5034082946835579}]
["REIKU-G","PMWVG-17P16",null,null,30,4.5937345355511363,{"$f":"F571*(1-Elteq!$F$8)","v":4.5937345355511363}]
["REIKU-G","PMWVG-23M25",null,null,30,7.058350536366496,{"$f":"F572*(1-Elteq!$F$8)","v":7.058350536366496}]
["REIKU-G","PMWVG-23P21",null,null,30,7.8325754580885949,{"$f":"F573*(1-Elteq!$F$8)","v":7.8325754580885949}]
["REIKU-G","PMWVG-29M32",null,null,20,8.7616453641551164,{"$f":"F574*(1-Elteq!$F$8)","v":8.7616453641551164}]
["REIKU-G","PMWVG-29P29",null,null,20,8.7616453641551164,{"$f":"F575*(1-Elteq!$F$8)","v":8.7616453641551164}]
["REIKU-G","PMWVG-36M40",null,null,10,14.581236025766247,{"$f":"F576*(1-Elteq!$F$8)","v":14.581236025766247}]
["REIKU-G","PMWVG-36P36",null,null,10,14.465102287507936,{"$f":"F577*(1-Elteq!$F$8)","v":14.465102287507936}]
["REIKU-G","PMWVG-48M50",null,null,10,21.510549075179064,{"$f":"F578*(1-Elteq!$F$8)","v":21.510549075179064}]
["REIKU-G","PMWVG-48P48",null,null,10,21.265377849967059,{"$f":"F579*(1-Elteq!$F$8)","v":21.265377849967059}]
["REIKU-G","PSNOG-07M081",null,null,50,4.6324457816372417,{"$f":"F580*(1-Elteq!$F$8)","v":4.6324457816372417}]
["REIKU-G","PSNOG-07M121",null,null,50,4.6324457816372417,{"$f":"F581*(1-Elteq!$F$8)","v":4.6324457816372417}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-G"},"PWNOG-07M081",null,null,50,4.6324457816372417,{"$f":"F582*(1-Elteq!$F$8)","v":4.6324457816372417}]
["REIKU-G","PWNOG-07M121",null,null,50,4.6324457816372417,{"$f":"F583*(1-Elteq!$F$8)","v":4.6324457816372417}]
["REIKU-G","PWNOG-07M181",null,null,50,4.6324457816372417,{"$f":"F584*(1-Elteq!$F$8)","v":4.6324457816372417}]
["REIKU-G","PWNOG-07M301",null,null,50,4.8647132581538735,{"$f":"F585*(1-Elteq!$F$8)","v":4.8647132581538735}]
["REIKU-G","VMARG-10M16",null,null,30,3.9485471007827186,{"$f":"F586*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-G","VMARG-10M20",null,null,30,3.9485471007827186,{"$f":"F587*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-G","VMARG-10P09",null,null,30,3.9485471007827186,{"$f":"F588*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-G","VMARG-12M16",null,null,30,3.9485471007827186,{"$f":"F589*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-G","VMARG-12M20",null,null,30,3.9485471007827186,{"$f":"F590*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-G","VMARG-12P11",null,null,30,3.9485471007827186,{"$f":"F591*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-G","VMARG-17M20",null,null,30,4.8001945146770293,{"$f":"F592*(1-Elteq!$F$8)","v":4.8001945146770293}]
["REIKU-G","VMARG-17M25",null,null,30,4.8001945146770293,{"$f":"F593*(1-Elteq!$F$8)","v":4.8001945146770293}]
["REIKU-G","VMARG-17P13",null,null,30,4.8001945146770293,{"$f":"F594*(1-Elteq!$F$8)","v":4.8001945146770293}]
["REIKU-G","VMARG-17P16",null,null,30,4.8001945146770293,{"$f":"F595*(1-Elteq!$F$8)","v":4.8001945146770293}]
["REIKU-G","VMARG-23M32",null,null,30,7.2648105154923881,{"$f":"F596*(1-Elteq!$F$8)","v":7.2648105154923881}]
["REIKU-G","VMARG-23P21",null,null,30,7.2648105154923881,{"$f":"F597*(1-Elteq!$F$8)","v":7.2648105154923881}]
["REIKU-G","VMARG-29M32",null,null,30,8.7487416154597462,{"$f":"F598*(1-Elteq!$F$8)","v":8.7487416154597462}]
["REIKU-G","VMARG-29M40",null,null,20,8.7487416154597462,{"$f":"F599*(1-Elteq!$F$8)","v":8.7487416154597462}]
["REIKU-G","VMARG-29P29",null,null,20,8.7487416154597462,{"$f":"F600*(1-Elteq!$F$8)","v":8.7487416154597462}]
["REIKU-G","VMARG-36M40",null,null,10,15.265134706620771,{"$f":"F601*(1-Elteq!$F$8)","v":15.265134706620771}]
["REIKU-G","VMARG-36M50",null,null,10,15.265134706620771,{"$f":"F602*(1-Elteq!$F$8)","v":15.265134706620771}]
["REIKU-G","VMARG-36P36",null,null,10,15.265134706620771,{"$f":"F603*(1-Elteq!$F$8)","v":15.265134706620771}]
["REIKU-G","VMARG-48M63",null,null,10,20.775035399543064,{"$f":"F604*(1-Elteq!$F$8)","v":20.775035399543064}]
["REIKU-G","VMARG-48P48",null,null,10,20.775035399543064,{"$f":"F605*(1-Elteq!$F$8)","v":20.775035399543064}]
["REIKU-G","VMAVG-10M16",null,null,30,4.1291995825178764,{"$f":"F606*(1-Elteq!$F$8)","v":4.1291995825178764}]
["REIKU-G","VMAVG-10M20",null,null,30,4.1679108286039801,{"$f":"F607*(1-Elteq!$F$8)","v":4.1679108286039801}]
["REIKU-G","VMAVG-10P09",null,null,30,4.1162958338225071,{"$f":"F608*(1-Elteq!$F$8)","v":4.1162958338225071}]
["REIKU-G","VMAVG-12M16",null,null,30,4.1162958338225071,{"$f":"F609*(1-Elteq!$F$8)","v":4.1162958338225071}]
["REIKU-G","VMAVG-12M20",null,null,30,4.1679108286039801,{"$f":"F610*(1-Elteq!$F$8)","v":4.1679108286039801}]
["REIKU-G","VMAVG-12P11",null,null,30,4.1291995825178764,{"$f":"F611*(1-Elteq!$F$8)","v":4.1291995825178764}]
["REIKU-G","VMAVG-17M20",null,null,30,5.0066544938029232,{"$f":"F612*(1-Elteq!$F$8)","v":5.0066544938029232}]
["REIKU-G","VMAVG-17M25",null,null,30,5.0453657398890277,{"$f":"F613*(1-Elteq!$F$8)","v":5.0453657398890277}]
["REIKU-G","VMAVG-17P13",null,null,30,4.9808469964121862,{"$f":"F614*(1-Elteq!$F$8)","v":4.9808469964121862}]
["REIKU-G","VMAVG-17P16",null,null,30,4.9937507451075573,{"$f":"F615*(1-Elteq!$F$8)","v":4.9937507451075573}]
["REIKU-G","VMAVG-23M32",null,null,30,7.5874042328765983,{"$f":"F616*(1-Elteq!$F$8)","v":7.5874042328765983}]
["REIKU-G","VMAVG-23P21",null,null,30,7.4970779920090189,{"$f":"F617*(1-Elteq!$F$8)","v":7.4970779920090189}]
["REIKU-G","VMBVG-29M32",null,null,20,9.084239081539323,{"$f":"F618*(1-Elteq!$F$8)","v":9.084239081539323}]
["REIKU-G","VMAVB-29M32",null,null,20,9.084239081539323,{"$f":"F619*(1-Elteq!$F$8)","v":9.084239081539323}]
["REIKU-G","VMAVG-29M40",null,null,20,9.2390840658837483,{"$f":"F620*(1-Elteq!$F$8)","v":9.2390840658837483}]
["REIKU-G","VMAVG-29P29",null,null,20,9.0713353328439563,{"$f":"F621*(1-Elteq!$F$8)","v":9.0713353328439563}]
["REIKU-G","VMAVG-36M40",null,null,10,15.768380905740136,{"$f":"F622*(1-Elteq!$F$8)","v":15.768380905740136}]
["REIKU-G","VMAVG-36M50",null,null,10,15.974840884866033,{"$f":"F623*(1-Elteq!$F$8)","v":15.974840884866033}]
["REIKU-G","VMAVG-36P36",null,null,10,15.66515091617719,{"$f":"F624*(1-Elteq!$F$8)","v":15.66515091617719}]
["REIKU-G","VMAVG-48M63",null,null,10,21.717009054304945,{"$f":"F625*(1-Elteq!$F$8)","v":21.717009054304945}]
["REIKU-G","VMAVG-48P48",null,null,10,21.252474101271687,{"$f":"F626*(1-Elteq!$F$8)","v":21.252474101271687}]
["REIKU-G","VMBRG-10M16",null,null,30,3.9485471007827186,{"$f":"F627*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-G","VMBRG-10M20",null,null,30,3.9485471007827186,{"$f":"F628*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-G","VMBRG-10P09",null,null,30,3.9485471007827186,{"$f":"F629*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-G","VMBRG-10P11",null,null,30,3.9485471007827186,{"$f":"F630*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-G","VMBRG-10P13",null,null,30,3.9485471007827186,{"$f":"F631*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-G","VMBRG-12M16",null,null,30,3.9485471007827186,{"$f":"F632*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-G","VMBRG-12M20",null,null,30,3.9485471007827186,{"$f":"F633*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-G","VMBRG-12P11",null,null,30,3.9485471007827186,{"$f":"F634*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-G","VMBRG-12P13",null,null,30,3.9485471007827186,{"$f":"F635*(1-Elteq!$F$8)","v":3.9485471007827186}]
["REIKU-G","VMBRG-17M20",null,null,30,4.8001945146770293,{"$f":"F636*(1-Elteq!$F$8)","v":4.8001945146770293}]
["REIKU-G","VMBRG-17M25",null,null,30,4.8001945146770293,{"$f":"F637*(1-Elteq!$F$8)","v":4.8001945146770293}]
["REIKU-G","VMBRG-17P13",null,null,30,4.8001945146770293,{"$f":"F638*(1-Elteq!$F$8)","v":4.8001945146770293}]
["REIKU-G","VMBRG-17P16",null,null,30,4.8001945146770293,{"$f":"F639*(1-Elteq!$F$8)","v":4.8001945146770293}]
["REIKU-G","VMBRG-23M32",null,null,30,7.2648105154923881,{"$f":"F640*(1-Elteq!$F$8)","v":7.2648105154923881}]
["REIKU-G","VMBRG-23P21",null,null,30,7.2648105154923881,{"$f":"F641*(1-Elteq!$F$8)","v":7.2648105154923881}]
["REIKU-G","VMBRG-29M32",null,null,20,8.7487416154597462,{"$f":"F642*(1-Elteq!$F$8)","v":8.7487416154597462}]
["REIKU-G","VMBRG-29M40",null,null,20,8.7487416154597462,{"$f":"F643*(1-Elteq!$F$8)","v":8.7487416154597462}]
["REIKU-G","VMBRG-29P29",null,null,20,8.7487416154597462,{"$f":"F644*(1-Elteq!$F$8)","v":8.7487416154597462}]
["REIKU-G","VMBRG-36M40",null,null,10,15.265134706620771,{"$f":"F645*(1-Elteq!$F$8)","v":15.265134706620771}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-G"},"VMBRG-36M50",null,null,10,15.265134706620771,{"$f":"F646*(1-Elteq!$F$8)","v":15.265134706620771}]
["REIKU-G","VMBRG-36P36",null,null,10,15.265134706620771,{"$f":"F647*(1-Elteq!$F$8)","v":15.265134706620771}]
["REIKU-G","VMBRG-48M63",null,null,10,20.775035399543064,{"$f":"F648*(1-Elteq!$F$8)","v":20.775035399543064}]
["REIKU-G","VMBRG-48P48",null,null,10,20.775035399543064,{"$f":"F649*(1-Elteq!$F$8)","v":20.775035399543064}]
["REIKU-G","VMBVG-10M16",null,null,30,4.1291995825178764,{"$f":"F650*(1-Elteq!$F$8)","v":4.1291995825178764}]
["REIKU-G","VMBVG-10M20",null,null,30,4.1679108286039801,{"$f":"F651*(1-Elteq!$F$8)","v":4.1679108286039801}]
["REIKU-G","VMBVG-10P09",null,null,30,4.1162958338225071,{"$f":"F652*(1-Elteq!$F$8)","v":4.1162958338225071}]
["REIKU-G","VMBVG-10P11",null,null,30,4.1291995825178764,{"$f":"F653*(1-Elteq!$F$8)","v":4.1291995825178764}]
["REIKU-G","VMBVG-10P13",null,null,30,4.142103331213244,{"$f":"F654*(1-Elteq!$F$8)","v":4.142103331213244}]
["REIKU-G","VMBVG-12M16",null,null,30,4.1162958338225071,{"$f":"F655*(1-Elteq!$F$8)","v":4.1162958338225071}]
["REIKU-G","VMBVG-12M20",null,null,30,4.1679108286039801,{"$f":"F656*(1-Elteq!$F$8)","v":4.1679108286039801}]
["REIKU-G","VMBVG-12P11",null,null,30,4.1291995825178764,{"$f":"F657*(1-Elteq!$F$8)","v":4.1291995825178764}]
["REIKU-G","VMBVG-12P13",null,null,30,4.142103331213244,{"$f":"F658*(1-Elteq!$F$8)","v":4.142103331213244}]
["REIKU-G","VMBVG-17M20",null,null,30,5.0066544938029232,{"$f":"F659*(1-Elteq!$F$8)","v":5.0066544938029232}]
["REIKU-G","VMBVG-17M25",null,null,30,5.0453657398890277,{"$f":"F660*(1-Elteq!$F$8)","v":5.0453657398890277}]
["REIKU-G","VMBVG-17P13",null,null,30,4.9808469964121862,{"$f":"F661*(1-Elteq!$F$8)","v":4.9808469964121862}]
["REIKU-G","VMBVG-17P16",null,null,30,4.9937507451075573,{"$f":"F662*(1-Elteq!$F$8)","v":4.9937507451075573}]
["REIKU-G","VMBVG-23M32",null,null,30,7.5874042328765983,{"$f":"F663*(1-Elteq!$F$8)","v":7.5874042328765983}]
["REIKU-G","VMBVG-23P21",null,null,30,7.4970779920090189,{"$f":"F664*(1-Elteq!$F$8)","v":7.4970779920090189}]
["REIKU-G","VMBVG-29M40",null,null,20,9.2390840658837483,{"$f":"F665*(1-Elteq!$F$8)","v":9.2390840658837483}]
["REIKU-G","VMBVG-29P29",null,null,20,9.0713353328439563,{"$f":"F666*(1-Elteq!$F$8)","v":9.0713353328439563}]
["REIKU-G","VMBVG-36M40",null,null,10,15.768380905740136,{"$f":"F667*(1-Elteq!$F$8)","v":15.768380905740136}]
["REIKU-G","VMBVG-36M50",null,null,10,15.974840884866033,{"$f":"F668*(1-Elteq!$F$8)","v":15.974840884866033}]
["REIKU-G","VMBVG-36P36",null,null,10,15.66515091617719,{"$f":"F669*(1-Elteq!$F$8)","v":15.66515091617719}]
["REIKU-G","VMBVG-48M63",null,null,10,21.717009054304945,{"$f":"F670*(1-Elteq!$F$8)","v":21.717009054304945}]
["REIKU-G","VMBVG-48P48",null,null,10,21.252474101271687,{"$f":"F671*(1-Elteq!$F$8)","v":21.252474101271687}]
["REIKU-G","VMGRG-10M16",null,null,30,3.0194771947161958,{"$f":"F672*(1-Elteq!$F$8)","v":3.0194771947161958}]
["REIKU-G","VMGRG-10M20",null,null,30,3.0194771947161958,{"$f":"F673*(1-Elteq!$F$8)","v":3.0194771947161958}]
["REIKU-G","VMGRG-10P09",null,null,30,3.0194771947161958,{"$f":"F674*(1-Elteq!$F$8)","v":3.0194771947161958}]
["REIKU-G","VMGRG-12M16",null,null,30,3.5227233938355633,{"$f":"F675*(1-Elteq!$F$8)","v":3.5227233938355633}]
["REIKU-G","VMGRG-12M20",null,null,30,3.5227233938355633,{"$f":"F676*(1-Elteq!$F$8)","v":3.5227233938355633}]
["REIKU-G","VMGRG-12P11",null,null,30,3.5227233938355633,{"$f":"F677*(1-Elteq!$F$8)","v":3.5227233938355633}]
["REIKU-G","VMGRG-17M20",null,null,30,4.2195258233854531,{"$f":"F678*(1-Elteq!$F$8)","v":4.2195258233854531}]
["REIKU-G","VMGRG-17M25",null,null,30,4.2195258233854531,{"$f":"F679*(1-Elteq!$F$8)","v":4.2195258233854531}]
["REIKU-G","VMGRG-17P13",null,null,30,4.1808145772993504,{"$f":"F680*(1-Elteq!$F$8)","v":4.1808145772993504}]
["REIKU-G","VMGRG-17P16",null,null,30,4.2195258233854531,{"$f":"F681*(1-Elteq!$F$8)","v":4.2195258233854531}]
["REIKU-G","VMGRG-23M25",null,null,30,7.1873880233201763,{"$f":"F682*(1-Elteq!$F$8)","v":7.1873880233201763}]
["REIKU-G","VMGRG-23M32",null,null,30,7.1873880233201763,{"$f":"F683*(1-Elteq!$F$8)","v":7.1873880233201763}]
["REIKU-G","VMGRG-23P21",null,null,30,7.1873880233201763,{"$f":"F684*(1-Elteq!$F$8)","v":7.1873880233201763}]
["REIKU-G","VMGRG-29M32",null,null,20,8.5680891337245928,{"$f":"F685*(1-Elteq!$F$8)","v":8.5680891337245928}]
["REIKU-G","VMGRG-29M40",null,null,20,8.5680891337245928,{"$f":"F686*(1-Elteq!$F$8)","v":8.5680891337245928}]
["REIKU-G","VMGRG-29P29",null,null,20,8.5680891337245928,{"$f":"F687*(1-Elteq!$F$8)","v":8.5680891337245928}]
["REIKU-G","VMGRG-36M40",null,null,10,13.716684863176566,{"$f":"F688*(1-Elteq!$F$8)","v":13.716684863176566}]
["REIKU-G","VMGRG-36M50",null,null,10,13.716684863176566,{"$f":"F689*(1-Elteq!$F$8)","v":13.716684863176566}]
["REIKU-G","VMGRG-36P36",null,null,10,13.716684863176566,{"$f":"F690*(1-Elteq!$F$8)","v":13.716684863176566}]
["REIKU-G","VMGRG-48M63",null,null,10,16.723258309197401,{"$f":"F691*(1-Elteq!$F$8)","v":16.723258309197401}]
["REIKU-G","VMGRG-48P48",null,null,10,16.723258309197401,{"$f":"F692*(1-Elteq!$F$8)","v":16.723258309197401}]
["REIKU-G","VMGVG-10M16",null,null,30,3.1872259277559856,{"$f":"F693*(1-Elteq!$F$8)","v":3.1872259277559856}]
["REIKU-G","VMGVG-10M16Z",null,null,30,6.9551205468035464,{"$f":"F694*(1-Elteq!$F$8)","v":6.9551205468035464}]
["REIKU-G","VMGVG-10M20",null,null,30,3.2259371738420892,{"$f":"F695*(1-Elteq!$F$8)","v":3.2259371738420892}]
["REIKU-G","VMGVG-10P09",null,null,30,3.1872259277559856,{"$f":"F696*(1-Elteq!$F$8)","v":3.1872259277559856}]
["REIKU-G","VMGVG-12M16",null,null,30,3.6904721268753504,{"$f":"F697*(1-Elteq!$F$8)","v":3.6904721268753504}]
["REIKU-G","VMGVG-12M16Z",null,null,30,8.0519391859098572,{"$f":"F698*(1-Elteq!$F$8)","v":8.0519391859098572}]
["REIKU-G","VMGVG-12M20",null,null,30,3.7291833729614554,{"$f":"F699*(1-Elteq!$F$8)","v":3.7291833729614554}]
["REIKU-G","VMGVG-12M20Z",null,null,30,9.0584315841485932,{"$f":"F700*(1-Elteq!$F$8)","v":9.0584315841485932}]
["REIKU-G","VMGVG-12P11",null,null,30,3.7033758755707202,{"$f":"F701*(1-Elteq!$F$8)","v":3.7033758755707202}]
["REIKU-G","VMGVG-17M20",null,null,30,4.425985802511347,{"$f":"F702*(1-Elteq!$F$8)","v":4.425985802511347}]
["REIKU-G","VMGVG-17M20Z",null,null,30,16.387760843117825,{"$f":"F703*(1-Elteq!$F$8)","v":16.387760843117825}]
["REIKU-G","VMGVG-17M25",null,null,30,4.4517932999020848,{"$f":"F704*(1-Elteq!$F$8)","v":4.4517932999020848}]
["REIKU-G","VMGVG-17P13",null,null,30,4.3743708077298731,{"$f":"F705*(1-Elteq!$F$8)","v":4.3743708077298731}]
["REIKU-G","VMGVG-17P16",null,null,30,4.425985802511347,{"$f":"F706*(1-Elteq!$F$8)","v":4.425985802511347}]
["REIKU-G","VMGVG-23M25",null,null,30,7.4196554998368081,{"$f":"F707*(1-Elteq!$F$8)","v":7.4196554998368081}]
["REIKU-G","VMGVG-23M25Z",null,null,30,19.626601765655273,{"$f":"F708*(1-Elteq!$F$8)","v":19.626601765655273}]
["REIKU-G","VMGVG-23M32",null,null,30,7.5099817407043883,{"$f":"F709*(1-Elteq!$F$8)","v":7.5099817407043883}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-G"},"VMGVG-23P21",null,null,30,7.4454629972275459,{"$f":"F710*(1-Elteq!$F$8)","v":7.4454629972275459}]
["REIKU-G","VMGVG-29M32",null,null,20,8.9035865998041697,{"$f":"F711*(1-Elteq!$F$8)","v":8.9035865998041697}]
["REIKU-G","VMGVG-29M32Z",null,null,20,25.665556155087671,{"$f":"F712*(1-Elteq!$F$8)","v":25.665556155087671}]
["REIKU-G","VMGVG-29M40",null,null,20,9.0713353328439563,{"$f":"F713*(1-Elteq!$F$8)","v":9.0713353328439563}]
["REIKU-G","VMGVG-29P29",null,null,20,8.9035865998041697,{"$f":"F714*(1-Elteq!$F$8)","v":8.9035865998041697}]
["REIKU-G","VMGVG-36M40",null,null,10,14.219931062295936,{"$f":"F715*(1-Elteq!$F$8)","v":14.219931062295936}]
["REIKU-G","VMGVG-36M40Z",null,null,10,34.1304152992493,{"$f":"F716*(1-Elteq!$F$8)","v":34.1304152992493}]
["REIKU-G","VMGVG-36M50",null,null,10,14.426391041421827,{"$f":"F717*(1-Elteq!$F$8)","v":14.426391041421827}]
["REIKU-G","VMGVG-36P36",null,null,10,14.116701072732992,{"$f":"F718*(1-Elteq!$F$8)","v":14.116701072732992}]
["REIKU-G","VMGVG-48M63",null,null,10,17.652328215263921,{"$f":"F719*(1-Elteq!$F$8)","v":17.652328215263921}]
["REIKU-G","VMGVG-48M63Z",null,null,10,51.31820856147997,{"$f":"F720*(1-Elteq!$F$8)","v":51.31820856147997}]
["REIKU-G","VMGVG-48P48",null,null,10,17.213600759621389,{"$f":"F721*(1-Elteq!$F$8)","v":17.213600759621389}]
["REIKU-G","VMSVG-12/18",null,null,30,7.4841742433136487,{"$f":"F722*(1-Elteq!$F$8)","v":7.4841742433136487}]
["REIKU-G","VMSVG-17/20",null,null,30,7.5357892380951208,{"$f":"F723*(1-Elteq!$F$8)","v":7.5357892380951208}]
["REIKU-G","VMSVG-17/22",null,null,30,7.5357892380951208,{"$f":"F724*(1-Elteq!$F$8)","v":7.5357892380951208}]
["REIKU-G","VMSVG-17/25",null,null,30,7.5357892380951208,{"$f":"F725*(1-Elteq!$F$8)","v":7.5357892380951208}]
["REIKU-G","VMSVG-23/28",null,null,20,9.0326240867578527,{"$f":"F726*(1-Elteq!$F$8)","v":9.0326240867578527}]
["REIKU-G","VMSVG-29/32",null,null,20,11.252097224678849,{"$f":"F727*(1-Elteq!$F$8)","v":11.252097224678849}]
["REIKU-G","VMSVG-29/37",null,null,20,11.252068862361213,{"$f":"F728*(1-Elteq!$F$8)","v":11.252068862361213}]
["REIKU-G","VMSVG-36/40",null,null,10,14.310319269428401,{"$f":"F729*(1-Elteq!$F$8)","v":14.310319269428401}]
["REIKU-G","VMSVG-36/47",null,null,10,14.310257303163514,{"$f":"F730*(1-Elteq!$F$8)","v":14.310257303163514}]
["REIKU-G","VMSVG-48/59",null,null,10,20.658901661284748,{"$f":"F731*(1-Elteq!$F$8)","v":20.658901661284748}]
["REIKU-G","VPARG-10G01",null,null,50,2.6065572364644094,{"$f":"F732*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-G","VPARG-10M16",null,null,50,2.6065572364644094,{"$f":"F733*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-G","VPARG-10M20",null,null,50,2.6065572364644094,{"$f":"F734*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-G","VPARG-10P09",null,null,50,2.6065572364644094,{"$f":"F735*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-G","VPARG-12G01",null,null,50,2.7097872260273559,{"$f":"F736*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-G","VPARG-12M16",null,null,50,2.7097872260273559,{"$f":"F737*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-G","VPARG-12M20",null,null,50,2.7097872260273559,{"$f":"F738*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-G","VPARG-12P11",null,null,50,2.6323647338551464,{"$f":"F739*(1-Elteq!$F$8)","v":2.6323647338551464}]
["REIKU-G","VPARG-17G02",null,null,50,2.7097872260273559,{"$f":"F740*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-G","VPARG-17M20",null,null,50,2.7097872260273559,{"$f":"F741*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-G","VPARG-17M25",null,null,50,2.7097872260273559,{"$f":"F742*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-G","VPARG-17P16",null,null,50,2.7097872260273559,{"$f":"F743*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-G","VPARG-23G03",null,null,30,4.6840607764187148,{"$f":"F744*(1-Elteq!$F$8)","v":4.6840607764187148}]
["REIKU-G","VPARG-23M25",null,null,50,4.6840607764187148,{"$f":"F745*(1-Elteq!$F$8)","v":4.6840607764187148}]
["REIKU-G","VPARG-23M32",null,null,30,4.6840607764187148,{"$f":"F746*(1-Elteq!$F$8)","v":4.6840607764187148}]
["REIKU-G","VPARG-23P21",null,null,30,4.6840607764187148,{"$f":"F747*(1-Elteq!$F$8)","v":4.6840607764187148}]
["REIKU-G","VPARG-29G04",null,null,30,6.684141824200811,{"$f":"F748*(1-Elteq!$F$8)","v":6.684141824200811}]
["REIKU-G","VPARG-29M32",null,null,30,6.684141824200811,{"$f":"F749*(1-Elteq!$F$8)","v":6.684141824200811}]
["REIKU-G","VPARG-29M40",null,null,30,6.684141824200811,{"$f":"F750*(1-Elteq!$F$8)","v":6.684141824200811}]
["REIKU-G","VPARG-29P29",null,null,30,6.684141824200811,{"$f":"F751*(1-Elteq!$F$8)","v":6.684141824200811}]
["REIKU-G","VPARG-36G05",null,null,10,10.232672715427109,{"$f":"F752*(1-Elteq!$F$8)","v":10.232672715427109}]
["REIKU-G","VPARG-36M40",null,null,10,10.232672715427109,{"$f":"F753*(1-Elteq!$F$8)","v":10.232672715427109}]
["REIKU-G","VPARG-36M50",null,null,10,10.232672715427109,{"$f":"F754*(1-Elteq!$F$8)","v":10.232672715427109}]
["REIKU-G","VPARG-36P36",null,null,10,10.232672715427109,{"$f":"F755*(1-Elteq!$F$8)","v":10.232672715427109}]
["REIKU-G","VPARG-48G07",null,null,10,11.277876359751948,{"$f":"F756*(1-Elteq!$F$8)","v":11.277876359751948}]
["REIKU-G","VPARG-48M50",null,null,10,11.277876359751948,{"$f":"F757*(1-Elteq!$F$8)","v":11.277876359751948}]
["REIKU-G","VPARG-48M63",null,null,10,11.277876359751948,{"$f":"F758*(1-Elteq!$F$8)","v":11.277876359751948}]
["REIKU-G","VPARG-48P48",null,null,10,11.277876359751948,{"$f":"F759*(1-Elteq!$F$8)","v":11.277876359751948}]
["REIKU-G","VPAVG-10M16",null,null,50,2.7743059695041974,{"$f":"F760*(1-Elteq!$F$8)","v":2.7743059695041974}]
["REIKU-G","VPAVG-10M20",null,null,50,2.8130172155903033,{"$f":"F761*(1-Elteq!$F$8)","v":2.8130172155903033}]
["REIKU-G","VPAVG-10P09",null,null,50,2.7614022208088285,{"$f":"F762*(1-Elteq!$F$8)","v":2.7614022208088285}]
["REIKU-G","VPAVG-12M16",null,null,50,2.8775359590671443,{"$f":"F763*(1-Elteq!$F$8)","v":2.8775359590671443}]
["REIKU-G","VPAVG-12M20",null,null,50,2.9291509538486182,{"$f":"F764*(1-Elteq!$F$8)","v":2.9291509538486182}]
["REIKU-G","VPAVG-12P11",null,null,50,2.8001134668949357,{"$f":"F765*(1-Elteq!$F$8)","v":2.8001134668949357}]
["REIKU-G","VPAVG-17M20",null,null,50,2.9291509538486182,{"$f":"F766*(1-Elteq!$F$8)","v":2.9291509538486182}]
["REIKU-G","VPAVG-17M25",null,null,50,2.9549584512393556,{"$f":"F767*(1-Elteq!$F$8)","v":2.9549584512393556}]
["REIKU-G","VPAVG-17P16",null,null,50,2.9162472051532493,{"$f":"F768*(1-Elteq!$F$8)","v":2.9162472051532493}]
["REIKU-G","VPAVG-23M25",null,null,30,4.9163282529353456,{"$f":"F769*(1-Elteq!$F$8)","v":4.9163282529353456}]
["REIKU-G","VPAVG-23M32",null,null,30,5.0066544938029232,{"$f":"F770*(1-Elteq!$F$8)","v":5.0066544938029232}]
["REIKU-G","VPAVG-23P21",null,null,30,4.9163282529353456,{"$f":"F771*(1-Elteq!$F$8)","v":4.9163282529353456}]
["REIKU-G","VPAVG-29M32",null,null,30,7.0067355415850194,{"$f":"F772*(1-Elteq!$F$8)","v":7.0067355415850194}]
["REIKU-G","VPAVG-29M40",null,null,30,7.1873880233201763,{"$f":"F773*(1-Elteq!$F$8)","v":7.1873880233201763}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-G"},"VPAVG-29P29",null,null,30,7.0067355415850194,{"$f":"F774*(1-Elteq!$F$8)","v":7.0067355415850194}]
["REIKU-G","VPAVG-36M40",null,null,10,10.735918914546478,{"$f":"F775*(1-Elteq!$F$8)","v":10.735918914546478}]
["REIKU-G","VPAVG-36M50",null,null,10,10.955282642367742,{"$f":"F776*(1-Elteq!$F$8)","v":10.955282642367742}]
["REIKU-G","VPAVG-36P36",null,null,10,10.63268892498353,{"$f":"F777*(1-Elteq!$F$8)","v":10.63268892498353}]
["REIKU-G","VPAVG-48M50",null,null,10,12.000486286692574,{"$f":"F778*(1-Elteq!$F$8)","v":12.000486286692574}]
["REIKU-G","VPAVG-48M63",null,null,10,12.21985001451384,{"$f":"F779*(1-Elteq!$F$8)","v":12.21985001451384}]
["REIKU-G","VPAVG-48P48",null,null,10,11.755315061480575,{"$f":"F780*(1-Elteq!$F$8)","v":11.755315061480575}]
["REIKU-G","VPBRG-10G01",null,null,50,2.6065572364644094,{"$f":"F781*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-G","VPBRG-10M16",null,null,50,2.6065572364644094,{"$f":"F782*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-G","VPBRG-10M20",null,null,50,2.6065572364644094,{"$f":"F783*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-G","VPBRG-10P09",null,null,50,2.6065572364644094,{"$f":"F784*(1-Elteq!$F$8)","v":2.6065572364644094}]
["REIKU-G","VPBRG-10P11",null,null,50,2.6839797286366194,{"$f":"F785*(1-Elteq!$F$8)","v":2.6839797286366194}]
["REIKU-G","VPBRG-10P13",null,null,50,2.6839797286366194,{"$f":"F786*(1-Elteq!$F$8)","v":2.6839797286366194}]
["REIKU-G","VPBRG-12G01",null,null,50,2.7097872260273559,{"$f":"F787*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-G","VPBRG-12M16",null,null,50,2.7097872260273559,{"$f":"F788*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-G","VPBRG-12M20",null,null,50,2.7097872260273559,{"$f":"F789*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-G","VPBRG-12P11",null,null,50,2.6323647338551464,{"$f":"F790*(1-Elteq!$F$8)","v":2.6323647338551464}]
["REIKU-G","VPBRG-12P13",null,null,50,2.7097872260273559,{"$f":"F791*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-G","VPBRG-17G02",null,null,50,2.7097872260273559,{"$f":"F792*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-G","VPBRG-17M20",null,null,50,2.7097872260273559,{"$f":"F793*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-G","VPBRG-17M25",null,null,50,2.7097872260273559,{"$f":"F794*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-G","VPBRG-17P13",null,null,50,2.7097872260273559,{"$f":"F795*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-G","VPBRG-17P16",null,null,50,2.7097872260273559,{"$f":"F796*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-G","VPBRG-23G03",null,null,30,4.6840607764187148,{"$f":"F797*(1-Elteq!$F$8)","v":4.6840607764187148}]
["REIKU-G","VPBRG-23M25",null,null,30,4.6840607764187148,{"$f":"F798*(1-Elteq!$F$8)","v":4.6840607764187148}]
["REIKU-G","VPBRG-23M32",null,null,30,4.6840607764187148,{"$f":"F799*(1-Elteq!$F$8)","v":4.6840607764187148}]
["REIKU-G","VPBRG-23P21",null,null,30,4.6840607764187148,{"$f":"F800*(1-Elteq!$F$8)","v":4.6840607764187148}]
["REIKU-G","VPBRG-29G04",null,null,30,6.684141824200811,{"$f":"F801*(1-Elteq!$F$8)","v":6.684141824200811}]
["REIKU-G","VPBRG-29M32",null,null,30,6.684141824200811,{"$f":"F802*(1-Elteq!$F$8)","v":6.684141824200811}]
["REIKU-G","VPBRG-29M40",null,null,30,6.684141824200811,{"$f":"F803*(1-Elteq!$F$8)","v":6.684141824200811}]
["REIKU-G","VPBRG-29P29",null,null,30,6.684141824200811,{"$f":"F804*(1-Elteq!$F$8)","v":6.684141824200811}]
["REIKU-G","VPBRG-36G05",null,null,10,10.232672715427109,{"$f":"F805*(1-Elteq!$F$8)","v":10.232672715427109}]
["REIKU-G","VPBRG-36M40",null,null,10,10.232672715427109,{"$f":"F806*(1-Elteq!$F$8)","v":10.232672715427109}]
["REIKU-G","VPBRG-36M50",null,null,10,10.232672715427109,{"$f":"F807*(1-Elteq!$F$8)","v":10.232672715427109}]
["REIKU-G","VPBRG-36P36",null,null,10,10.232672715427109,{"$f":"F808*(1-Elteq!$F$8)","v":10.232672715427109}]
["REIKU-G","VPBRG-48G07",null,null,10,11.277876359751948,{"$f":"F809*(1-Elteq!$F$8)","v":11.277876359751948}]
["REIKU-G","VPBRG-48M50",null,null,10,11.277876359751948,{"$f":"F810*(1-Elteq!$F$8)","v":11.277876359751948}]
["REIKU-G","VPBRG-48M63",null,null,10,11.277876359751948,{"$f":"F811*(1-Elteq!$F$8)","v":11.277876359751948}]
["REIKU-G","VPBRG-48P48",null,null,10,11.277876359751948,{"$f":"F812*(1-Elteq!$F$8)","v":11.277876359751948}]
["REIKU-G","VPBVG-10M16",null,null,50,2.7743059695041974,{"$f":"F813*(1-Elteq!$F$8)","v":2.7743059695041974}]
["REIKU-G","VPBVG-10M20",null,null,50,2.8130172155903033,{"$f":"F814*(1-Elteq!$F$8)","v":2.8130172155903033}]
["REIKU-G","VPBVG-10P09",null,null,50,2.7614022208088285,{"$f":"F815*(1-Elteq!$F$8)","v":2.7614022208088285}]
["REIKU-G","VPBVG-10P11",null,null,50,2.8517284616764083,{"$f":"F816*(1-Elteq!$F$8)","v":2.8517284616764083}]
["REIKU-G","VPBVG-10P13",null,null,50,2.8646322103717763,{"$f":"F817*(1-Elteq!$F$8)","v":2.8646322103717763}]
["REIKU-G","VPBVG-12M16",null,null,50,2.8775359590671443,{"$f":"F818*(1-Elteq!$F$8)","v":2.8775359590671443}]
["REIKU-G","VPBVG-12M20",null,null,50,2.9291509538486182,{"$f":"F819*(1-Elteq!$F$8)","v":2.9291509538486182}]
["REIKU-G","VPBVG-12P11",null,null,50,2.8001134668949357,{"$f":"F820*(1-Elteq!$F$8)","v":2.8001134668949357}]
["REIKU-G","VPBVG-12P13",null,null,50,2.8904397077625124,{"$f":"F821*(1-Elteq!$F$8)","v":2.8904397077625124}]
["REIKU-G","VPBVG-17M20",null,null,50,2.9291509538486182,{"$f":"F822*(1-Elteq!$F$8)","v":2.9291509538486182}]
["REIKU-G","VPBVG-17M25",null,null,50,2.9549584512393556,{"$f":"F823*(1-Elteq!$F$8)","v":2.9549584512393556}]
["REIKU-G","VPBVG-17P13",null,null,50,2.8904397077625124,{"$f":"F824*(1-Elteq!$F$8)","v":2.8904397077625124}]
["REIKU-G","VPBVG-17P16",null,null,50,2.9162472051532493,{"$f":"F825*(1-Elteq!$F$8)","v":2.9162472051532493}]
["REIKU-G","VPBVG-23M25",null,null,30,4.9163282529353456,{"$f":"F826*(1-Elteq!$F$8)","v":4.9163282529353456}]
["REIKU-G","VPBVG-23M32",null,null,30,5.0066544938029232,{"$f":"F827*(1-Elteq!$F$8)","v":5.0066544938029232}]
["REIKU-G","VPBVG-23P21",null,null,30,4.9163282529353456,{"$f":"F828*(1-Elteq!$F$8)","v":4.9163282529353456}]
["REIKU-G","VPBVG-29M32",null,null,30,7.0067355415850194,{"$f":"F829*(1-Elteq!$F$8)","v":7.0067355415850194}]
["REIKU-G","VPBVG-29M40",null,null,30,7.1873880233201763,{"$f":"F830*(1-Elteq!$F$8)","v":7.1873880233201763}]
["REIKU-G","VPBVG-29P29",null,null,30,7.0067355415850194,{"$f":"F831*(1-Elteq!$F$8)","v":7.0067355415850194}]
["REIKU-G","VPBVG-36M40",null,null,10,10.735918914546478,{"$f":"F832*(1-Elteq!$F$8)","v":10.735918914546478}]
["REIKU-G","VPBVG-36M50",null,null,10,10.955282642367742,{"$f":"F833*(1-Elteq!$F$8)","v":10.955282642367742}]
["REIKU-G","VPBVG-36P36",null,null,10,10.63268892498353,{"$f":"F834*(1-Elteq!$F$8)","v":10.63268892498353}]
["REIKU-G","VPBVG-48M50",null,null,10,12.000486286692574,{"$f":"F835*(1-Elteq!$F$8)","v":12.000486286692574}]
["REIKU-G","VPBVG-48M63",null,null,10,12.21985001451384,{"$f":"F836*(1-Elteq!$F$8)","v":12.21985001451384}]
["REIKU-G","VPBVG-48P48",null,null,10,11.755315061480575,{"$f":"F837*(1-Elteq!$F$8)","v":11.755315061480575}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-G"},"VPGRG-10G00",null,null,50,1.4581236025766247,{"$f":"F838*(1-Elteq!$F$8)","v":1.4581236025766247}]
["REIKU-G","VPGRG-10M12",null,null,50,1.4581236025766247,{"$f":"F839*(1-Elteq!$F$8)","v":1.4581236025766247}]
["REIKU-G","VPGRG-10M16",null,null,50,1.4581236025766247,{"$f":"F840*(1-Elteq!$F$8)","v":1.4581236025766247}]
["REIKU-G","VPGRG-10M16Z",null,null,30,3.6130496347031409,{"$f":"F841*(1-Elteq!$F$8)","v":3.6130496347031409}]
["REIKU-G","VPGRG-10M20",null,null,50,1.4581236025766247,{"$f":"F842*(1-Elteq!$F$8)","v":1.4581236025766247}]
["REIKU-G","VPGRG-10P07",null,null,50,1.4581236025766247,{"$f":"F843*(1-Elteq!$F$8)","v":1.4581236025766247}]
["REIKU-G","VPGRG-10P09",null,null,50,1.4581236025766247,{"$f":"F844*(1-Elteq!$F$8)","v":1.4581236025766247}]
["REIKU-G","VPGRG-10P11",null,null,50,1.4581236025766247,{"$f":"F845*(1-Elteq!$F$8)","v":1.4581236025766247}]
["REIKU-G","VPGRG-10P13",null,null,50,1.4581236025766247,{"$f":"F846*(1-Elteq!$F$8)","v":1.4581236025766247}]
["REIKU-G","VPGRG-12G01",null,null,50,1.4710273512719934,{"$f":"F847*(1-Elteq!$F$8)","v":1.4710273512719934}]
["REIKU-G","VPGRG-12G02",null,null,50,1.4710273512719934,{"$f":"F848*(1-Elteq!$F$8)","v":1.4710273512719934}]
["REIKU-G","VPGRG-12M16",null,null,50,1.4710273512719934,{"$f":"F849*(1-Elteq!$F$8)","v":1.4710273512719934}]
["REIKU-G","VPGRG-12M16Z",null,null,30,3.7937021164382991,{"$f":"F850*(1-Elteq!$F$8)","v":3.7937021164382991}]
["REIKU-G","VPGRG-12M20",null,null,50,1.4710273512719934,{"$f":"F851*(1-Elteq!$F$8)","v":1.4710273512719934}]
["REIKU-G","VPGRG-12M20Z",null,null,30,3.7937021164382991,{"$f":"F852*(1-Elteq!$F$8)","v":3.7937021164382991}]
["REIKU-G","VPGRG-12P09",null,null,50,1.4710273512719934,{"$f":"F853*(1-Elteq!$F$8)","v":1.4710273512719934}]
["REIKU-G","VPGRG-12P11",null,null,50,1.4710273512719934,{"$f":"F854*(1-Elteq!$F$8)","v":1.4710273512719934}]
["REIKU-G","VPGRG-12P13",null,null,50,1.4710273512719934,{"$f":"F855*(1-Elteq!$F$8)","v":1.4710273512719934}]
["REIKU-G","VPGRG-17G02",null,null,50,1.4839310999673616,{"$f":"F856*(1-Elteq!$F$8)","v":1.4839310999673616}]
["REIKU-G","VPGRG-17M20",null,null,50,1.4839310999673616,{"$f":"F857*(1-Elteq!$F$8)","v":1.4839310999673616}]
["REIKU-G","VPGRG-17M20Z",null,null,30,4.5163120433789263,{"$f":"F858*(1-Elteq!$F$8)","v":4.5163120433789263}]
["REIKU-G","VPGRG-17M25",null,null,50,1.4839310999673616,{"$f":"F859*(1-Elteq!$F$8)","v":1.4839310999673616}]
["REIKU-G","VPGRG-17M32",null,null,50,1.5742573408349396,{"$f":"F860*(1-Elteq!$F$8)","v":1.5742573408349396}]
["REIKU-G","VPGRG-17P11",null,null,50,1.4839310999673616,{"$f":"F861*(1-Elteq!$F$8)","v":1.4839310999673616}]
["REIKU-G","VPGRG-17P13",null,null,50,1.4839310999673616,{"$f":"F862*(1-Elteq!$F$8)","v":1.4839310999673616}]
["REIKU-G","VPGRG-17P16",null,null,50,1.4839310999673616,{"$f":"F863*(1-Elteq!$F$8)","v":1.4839310999673616}]
["REIKU-G","VPGRG-17P21",null,null,50,1.9484660530006226,{"$f":"F864*(1-Elteq!$F$8)","v":1.9484660530006226}]
["REIKU-G","VPGRG-23G03",null,null,30,2.4517122521199881,{"$f":"F865*(1-Elteq!$F$8)","v":2.4517122521199881}]
["REIKU-G","VPGRG-23M25",null,null,30,2.4517122521199881,{"$f":"F866*(1-Elteq!$F$8)","v":2.4517122521199881}]
["REIKU-G","VPGRG-23M25Z",null,null,30,5.4711894468361866,{"$f":"F867*(1-Elteq!$F$8)","v":5.4711894468361866}]
["REIKU-G","VPGRG-23M32",null,null,30,2.5162309955968301,{"$f":"F868*(1-Elteq!$F$8)","v":2.5162309955968301}]
["REIKU-G","VPGRG-23P16",null,null,50,2.4517122521199881,{"$f":"F869*(1-Elteq!$F$8)","v":2.4517122521199881}]
["REIKU-G","VPGRG-23P21",null,null,30,2.4517122521199881,{"$f":"F870*(1-Elteq!$F$8)","v":2.4517122521199881}]
["REIKU-G","VPGRG-29G04",null,null,30,3.1743221790606166,{"$f":"F871*(1-Elteq!$F$8)","v":3.1743221790606166}]
["REIKU-G","VPGRG-29M32",null,null,30,3.1743221790606166,{"$f":"F872*(1-Elteq!$F$8)","v":3.1743221790606166}]
["REIKU-G","VPGRG-29M32Z",null,null,20,7.2390030181016529,{"$f":"F873*(1-Elteq!$F$8)","v":7.2390030181016529}]
["REIKU-G","VPGRG-29M40",null,null,30,3.1743221790606166,{"$f":"F874*(1-Elteq!$F$8)","v":3.1743221790606166}]
["REIKU-G","VPGRG-29P29",null,null,30,3.1743221790606166,{"$f":"F875*(1-Elteq!$F$8)","v":3.1743221790606166}]
["REIKU-G","VPGRG-36G05",null,null,10,5.4066707033593433,{"$f":"F876*(1-Elteq!$F$8)","v":5.4066707033593433}]
["REIKU-G","VPGRG-36M40",null,null,10,5.4066707033593433,{"$f":"F877*(1-Elteq!$F$8)","v":5.4066707033593433}]
["REIKU-G","VPGRG-36M40Z",null,null,10,13.626358622308985,{"$f":"F878*(1-Elteq!$F$8)","v":13.626358622308985}]
["REIKU-G","VPGRG-36M50",null,null,10,5.4066707033593433,{"$f":"F879*(1-Elteq!$F$8)","v":5.4066707033593433}]
["REIKU-G","VPGRG-36P29",null,null,10,5.4066707033593433,{"$f":"F880*(1-Elteq!$F$8)","v":5.4066707033593433}]
["REIKU-G","VPGRG-36P36",null,null,10,5.4066707033593433,{"$f":"F881*(1-Elteq!$F$8)","v":5.4066707033593433}]
["REIKU-G","VPGRG-48G06",null,null,10,6.9938317928896518,{"$f":"F882*(1-Elteq!$F$8)","v":6.9938317928896518}]
["REIKU-G","VPGRG-48G07",null,null,10,6.9938317928896518,{"$f":"F883*(1-Elteq!$F$8)","v":6.9938317928896518}]
["REIKU-G","VPGRG-48M50",null,null,10,6.9938317928896518,{"$f":"F884*(1-Elteq!$F$8)","v":6.9938317928896518}]
["REIKU-G","VPGRG-48M63",null,null,10,6.9938317928896518,{"$f":"F885*(1-Elteq!$F$8)","v":6.9938317928896518}]
["REIKU-G","VPGRG-48M63Z",null,null,10,15.639343418786451,{"$f":"F886*(1-Elteq!$F$8)","v":15.639343418786451}]
["REIKU-G","VPGRG-48P42",null,null,10,6.9938317928896518,{"$f":"F887*(1-Elteq!$F$8)","v":6.9938317928896518}]
["REIKU-G","VPGRG-48P48",null,null,10,6.9938317928896518,{"$f":"F888*(1-Elteq!$F$8)","v":6.9938317928896518}]
["REIKU-G","VPGVG-10M12",null,null,50,1.6129685869210446,{"$f":"F889*(1-Elteq!$F$8)","v":1.6129685869210446}]
["REIKU-G","VPGVG-10M16",null,null,50,1.6258723356164138,{"$f":"F890*(1-Elteq!$F$8)","v":1.6258723356164138}]
["REIKU-G","VPGVG-10M20",null,null,50,1.6645835817025187,{"$f":"F891*(1-Elteq!$F$8)","v":1.6645835817025187}]
["REIKU-G","VPGVG-10P07",null,null,50,1.6129685869210446,{"$f":"F892*(1-Elteq!$F$8)","v":1.6129685869210446}]
["REIKU-G","VPGVG-10P09",null,null,50,1.6129685869210446,{"$f":"F893*(1-Elteq!$F$8)","v":1.6129685869210446}]
["REIKU-G","VPGVG-10P11",null,null,50,1.6258723356164138,{"$f":"F894*(1-Elteq!$F$8)","v":1.6258723356164138}]
["REIKU-G","VPGVG-10P13",null,null,50,1.638776084311782,{"$f":"F895*(1-Elteq!$F$8)","v":1.638776084311782}]
["REIKU-G","VPGVG-10S15",null,null,50,1.6258723356164138,{"$f":"F896*(1-Elteq!$F$8)","v":1.6258723356164138}]
["REIKU-G","VPGVG-12M16",null,null,50,1.638776084311782,{"$f":"F897*(1-Elteq!$F$8)","v":1.638776084311782}]
["REIKU-G","VPGVG-12M20",null,null,50,1.6774873303978866,{"$f":"F898*(1-Elteq!$F$8)","v":1.6774873303978866}]
["REIKU-G","VPGVG-12P09",null,null,50,1.6258723356164138,{"$f":"F899*(1-Elteq!$F$8)","v":1.6258723356164138}]
["REIKU-G","VPGVG-12P11",null,null,50,1.638776084311782,{"$f":"F900*(1-Elteq!$F$8)","v":1.638776084311782}]
["REIKU-G","VPGVG-12P13",null,null,50,1.65167983300715,{"$f":"F901*(1-Elteq!$F$8)","v":1.65167983300715}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-G"},"VPGVG-12S19",null,null,50,1.638776084311782,{"$f":"F902*(1-Elteq!$F$8)","v":1.638776084311782}]
["REIKU-G","VPGVG-17M20",null,null,50,1.6903910790932555,{"$f":"F903*(1-Elteq!$F$8)","v":1.6903910790932555}]
["REIKU-G","VPGVG-17M25",null,null,50,1.7161985764839915,{"$f":"F904*(1-Elteq!$F$8)","v":1.7161985764839915}]
["REIKU-G","VPGVG-17M32",null,null,50,1.9097548069145172,{"$f":"F905*(1-Elteq!$F$8)","v":1.9097548069145172}]
["REIKU-G","VPGVG-17P11",null,null,50,1.65167983300715,{"$f":"F906*(1-Elteq!$F$8)","v":1.65167983300715}]
["REIKU-G","VPGVG-17P13",null,null,50,1.6645835817025187,{"$f":"F907*(1-Elteq!$F$8)","v":1.6645835817025187}]
["REIKU-G","VPGVG-17P16",null,null,50,1.6774873303978866,{"$f":"F908*(1-Elteq!$F$8)","v":1.6774873303978866}]
["REIKU-G","VPGVG-17P21",null,null,50,2.1807335295172532,{"$f":"F909*(1-Elteq!$F$8)","v":2.1807335295172532}]
["REIKU-G","VPGVG-17S22",null,null,50,1.6903910790932555,{"$f":"F910*(1-Elteq!$F$8)","v":1.6903910790932555}]
["REIKU-G","VPGVG-23M25",null,null,30,2.6839797286366194,{"$f":"F911*(1-Elteq!$F$8)","v":2.6839797286366194}]
["REIKU-G","VPGVG-23M32",null,null,30,2.8388247129810407,{"$f":"F912*(1-Elteq!$F$8)","v":2.8388247129810407}]
["REIKU-G","VPGVG-23P16",null,null,50,2.6452684825505144,{"$f":"F913*(1-Elteq!$F$8)","v":2.6452684825505144}]
["REIKU-G","VPGVG-23P21",null,null,30,2.6839797286366194,{"$f":"F914*(1-Elteq!$F$8)","v":2.6839797286366194}]
["REIKU-G","VPGVG-23S28",null,null,30,2.7097872260273559,{"$f":"F915*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-G","VPGVG-23S32",null,null,30,2.7097872260273559,{"$f":"F916*(1-Elteq!$F$8)","v":2.7097872260273559}]
["REIKU-G","VPGVG-29M32",null,null,30,3.5098196451401935,{"$f":"F917*(1-Elteq!$F$8)","v":3.5098196451401935}]
["REIKU-G","VPGVG-29M40",null,null,30,3.6775683781799819,{"$f":"F918*(1-Elteq!$F$8)","v":3.6775683781799819}]
["REIKU-G","VPGVG-29P29",null,null,30,3.5098196451401935,{"$f":"F919*(1-Elteq!$F$8)","v":3.5098196451401935}]
["REIKU-G","VPGVG-29S37",null,null,30,3.5227233938355633,{"$f":"F920*(1-Elteq!$F$8)","v":3.5227233938355633}]
["REIKU-G","VPGVG-29S40",null,null,30,3.5227233938355633,{"$f":"F921*(1-Elteq!$F$8)","v":3.5227233938355633}]
["REIKU-G","VPGVG-36M40",null,null,10,5.9099169024787113,{"$f":"F922*(1-Elteq!$F$8)","v":5.9099169024787113}]
["REIKU-G","VPGVG-36M50",null,null,10,6.1292806302999709,{"$f":"F923*(1-Elteq!$F$8)","v":6.1292806302999709}]
["REIKU-G","VPGVG-36P29",null,null,10,5.7421681694389211,{"$f":"F924*(1-Elteq!$F$8)","v":5.7421681694389211}]
["REIKU-G","VPGVG-36P36",null,null,10,5.8066869129157617,{"$f":"F925*(1-Elteq!$F$8)","v":5.8066869129157617}]
["REIKU-G","VPGVG-48M50",null,null,10,7.7164417198302804,{"$f":"F926*(1-Elteq!$F$8)","v":7.7164417198302804}]
["REIKU-G","VPGVG-48M63",null,null,10,7.9358054476515418,{"$f":"F927*(1-Elteq!$F$8)","v":7.9358054476515418}]
["REIKU-G","VPGVG-48P42",null,null,10,8.0003241911283833,{"$f":"F928*(1-Elteq!$F$8)","v":8.0003241911283833}]
["REIKU-G","VPGVG-48P48",null,null,10,7.471270494618282,{"$f":"F929*(1-Elteq!$F$8)","v":7.471270494618282}]
["REIKU-G","VPIRG-10M121",null,null,50,2.0904072886496752,{"$f":"F930*(1-Elteq!$F$8)","v":2.0904072886496752}]
["REIKU-G","VPIRG-10M16",null,null,50,2.0904072886496752,{"$f":"F931*(1-Elteq!$F$8)","v":2.0904072886496752}]
["REIKU-G","VPIRG-10P07",null,null,50,2.0904072886496752,{"$f":"F932*(1-Elteq!$F$8)","v":2.0904072886496752}]
["REIKU-G","VPIRG-10P09",null,null,50,2.0904072886496752,{"$f":"F933*(1-Elteq!$F$8)","v":2.0904072886496752}]
["REIKU-G","VPIRG-10U05",null,null,50,2.464616000815357,{"$f":"F934*(1-Elteq!$F$8)","v":2.464616000815357}]
["REIKU-G","VPIRG-10U07",null,null,50,2.464616000815357,{"$f":"F935*(1-Elteq!$F$8)","v":2.464616000815357}]
["REIKU-G","VPIRG-12M16",null,null,50,2.1291185347357797,{"$f":"F936*(1-Elteq!$F$8)","v":2.1291185347357797}]
["REIKU-G","VPIRG-12M20",null,null,50,2.1291185347357797,{"$f":"F937*(1-Elteq!$F$8)","v":2.1291185347357797}]
["REIKU-G","VPIRG-12P11",null,null,50,2.1291185347357797,{"$f":"F938*(1-Elteq!$F$8)","v":2.1291185347357797}]
["REIKU-G","VPIRG-12P13",null,null,50,2.1291185347357797,{"$f":"F939*(1-Elteq!$F$8)","v":2.1291185347357797}]
["REIKU-G","VPIRG-12U05",null,null,50,2.5420384929875666,{"$f":"F940*(1-Elteq!$F$8)","v":2.5420384929875666}]
["REIKU-G","VPIRG-12U06",null,null,50,2.5420384929875666,{"$f":"F941*(1-Elteq!$F$8)","v":2.5420384929875666}]
["REIKU-G","VPIRG-12U07",null,null,50,2.5420384929875666,{"$f":"F942*(1-Elteq!$F$8)","v":2.5420384929875666}]
["REIKU-G","VPIRG-12U09",null,null,50,2.5420384929875666,{"$f":"F943*(1-Elteq!$F$8)","v":2.5420384929875666}]
["REIKU-G","VPIRG-12U10",null,null,50,2.5420384929875666,{"$f":"F944*(1-Elteq!$F$8)","v":2.5420384929875666}]
["REIKU-G","VPIRG-17M20",null,null,50,2.2065410269079901,{"$f":"F945*(1-Elteq!$F$8)","v":2.2065410269079901}]
["REIKU-G","VPIRG-17M25",null,null,50,2.2065410269079901,{"$f":"F946*(1-Elteq!$F$8)","v":2.2065410269079901}]
["REIKU-G","VPIRG-17P13",null,null,50,2.2065410269079901,{"$f":"F947*(1-Elteq!$F$8)","v":2.2065410269079901}]
["REIKU-G","VPIRG-17P16",null,null,50,2.2065410269079901,{"$f":"F948*(1-Elteq!$F$8)","v":2.2065410269079901}]
["REIKU-G","VPIRG-17U07",null,null,50,2.6194609851597779,{"$f":"F949*(1-Elteq!$F$8)","v":2.6194609851597779}]
["REIKU-G","VPIRG-17U09",null,null,50,2.6194609851597779,{"$f":"F950*(1-Elteq!$F$8)","v":2.6194609851597779}]
["REIKU-G","VPIRG-17U10",null,null,50,2.6194609851597779,{"$f":"F951*(1-Elteq!$F$8)","v":2.6194609851597779}]
["REIKU-G","VPIRG-17U11",null,null,50,2.6194609851597779,{"$f":"F952*(1-Elteq!$F$8)","v":2.6194609851597779}]
["REIKU-G","VPIRG-17U14",null,null,50,2.6194609851597779,{"$f":"F953*(1-Elteq!$F$8)","v":2.6194609851597779}]
["REIKU-G","VPIRG-17U17",null,null,50,2.6194609851597779,{"$f":"F954*(1-Elteq!$F$8)","v":2.6194609851597779}]
["REIKU-G","VPIRG-23M25",null,null,30,4.5292157920742966,{"$f":"F955*(1-Elteq!$F$8)","v":4.5292157920742966}]
["REIKU-G","VPIRG-23M32",null,null,30,4.5293102989558847,{"$f":"F956*(1-Elteq!$F$8)","v":4.5293102989558847}]
["REIKU-G","VPIRG-23P21",null,null,30,4.5292157920742966,{"$f":"F957*(1-Elteq!$F$8)","v":4.5292157920742966}]
["REIKU-G","VPIRG-23U14",null,null,30,5.4840931955315542,{"$f":"F958*(1-Elteq!$F$8)","v":5.4840931955315542}]
["REIKU-G","VPIRG-23U17",null,null,30,5.4840931955315542,{"$f":"F959*(1-Elteq!$F$8)","v":5.4840931955315542}]
["REIKU-G","VPIRG-23U18",null,null,30,5.4840931955315542,{"$f":"F960*(1-Elteq!$F$8)","v":5.4840931955315542}]
["REIKU-G","VPIRG-29M32",null,null,30,7.768056714611757,{"$f":"F961*(1-Elteq!$F$8)","v":7.768056714611757}]
["REIKU-G","VPIRG-29M40",null,null,30,7.7679821709365662,{"$f":"F962*(1-Elteq!$F$8)","v":7.7679821709365662}]
["REIKU-G","VPIRG-29P29",null,null,30,7.768056714611757,{"$f":"F963*(1-Elteq!$F$8)","v":7.768056714611757}]
["REIKU-G","VPIRG-29U24",null,null,30,9.3294103067513241,{"$f":"F964*(1-Elteq!$F$8)","v":9.3294103067513241}]
["REIKU-G","VPIRG-36M40",null,null,10,8.5035703902477469,{"$f":"F965*(1-Elteq!$F$8)","v":8.5035703902477469}]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"REIKU-G"},"VPIRG-36M50",null,null,10,8.5035781356397209,{"$f":"F966*(1-Elteq!$F$8)","v":8.5035781356397209}]
["REIKU-G","VPIRG-36P36",null,null,10,8.5035703902477469,{"$f":"F967*(1-Elteq!$F$8)","v":8.5035703902477469}]
["REIKU-G","VPIRG-48M50",null,null,10,15.381268444879082,{"$f":"F968*(1-Elteq!$F$8)","v":15.381268444879082}]
["REIKU-G","VPIRG-48M63",null,null,10,15.381236960090622,{"$f":"F969*(1-Elteq!$F$8)","v":15.381236960090622}]
["REIKU-G","VPIRG-48P48",null,null,10,15.381268444879082,{"$f":"F970*(1-Elteq!$F$8)","v":15.381268444879082}]
["REIKU-G","VPSRG-10M12",null,null,50,3.2646484199281942,{"$f":"F971*(1-Elteq!$F$8)","v":3.2646484199281942}]
["REIKU-G","VPSRG-10M16",null,null,50,3.2646484199281942,{"$f":"F972*(1-Elteq!$F$8)","v":3.2646484199281942}]
["REIKU-G","VPSRG-10M20",null,null,50,3.2646484199281942,{"$f":"F973*(1-Elteq!$F$8)","v":3.2646484199281942}]
["REIKU-G","VPSRG-12M20",null,null,50,3.380782158186511,{"$f":"F974*(1-Elteq!$F$8)","v":3.380782158186511}]
["REIKU-G","VPSVG-10M12",null,null,50,3.4194934042726155,{"$f":"F975*(1-Elteq!$F$8)","v":3.4194934042726155}]
["REIKU-G","VPSVG-10M16",null,null,50,3.4453009016633525,{"$f":"F976*(1-Elteq!$F$8)","v":3.4453009016633525}]
["REIKU-G","VPSVG-10M20",null,null,50,3.4840121477494579,{"$f":"F977*(1-Elteq!$F$8)","v":3.4840121477494579}]
["REIKU-G","VPSVG-12M20",null,null,50,3.6001458860077729,{"$f":"F978*(1-Elteq!$F$8)","v":3.6001458860077729}]

{"sheet":"TECHNIK","index":7,"n_rows":6604,"n_cols":8,"rows_kept":6604,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["sheetname","Objednávací kód",null,"Popis","Balenie","Cena za ks alebo m","Cena za kus po zľave","EAN"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"Cupal 0,5x500x2000",null,"Cupalový plech 0,5x500x2000mm, složení 70% Al + 30% Cu","1ks",168.119621007159,{"$f":"F5*(1-Elteq!$F$9)","v":168.119621007159},"8591735037079"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"Cupal 1,0x500x2000",null,"Cupalový plech 1,0x500x2000mm, složení 70% Al + 30% Cu","1ks",334.38361705838912,{"$f":"F6*(1-Elteq!$F$9)","v":334.38361705838912},"8591735031862"]
["TECHNIK","Cupal 1,5x500x2000",null,"Cupalový plech 1,5x500x2000mm, složení 70% Al + 30% Cu","1ks",503.61661303910546,{"$f":"F7*(1-Elteq!$F$9)","v":503.61661303910546},"8591735031879"]
["TECHNIK","Cupal 2,0x500x2000",null,"Cupalový plech 2,0x500x2000mm, složení 70% Al + 30% Cu","1ks",673.96298399337911,{"$f":"F8*(1-Elteq!$F$9)","v":673.96298399337911},"8591735031886"]
["TECHNIK","Cupal 25x100",null,"Cupalový pásek 1,0x250x1000mm, složení 70% Al + 30% Cu (dodáváno po 2ks)","1ks",100.01818512456811,{"$f":"F9*(1-Elteq!$F$9)","v":100.01818512456811},"8591735042394"]
["TECHNIK","Cupal 50x 3",null,"Cupalový pásek 1,0x500x30mm, složení 70% Al + 30% Cu","1ks",11.133749735573444,{"$f":"F10*(1-Elteq!$F$9)","v":11.133749735573444},"8591735050917"]
["TECHNIK","Cupal 50x 4",null,"Cupalový pásek 1,0x500x40mm, složení 70% Al + 30% Cu","1ks",14.102749665059696,{"$f":"F11*(1-Elteq!$F$9)","v":14.102749665059696},"8591735019372"]
["TECHNIK","Cupal 50x 4/0,5",null,"Cupalový pásek 0,5x500x40mm, složení 70% Al + 30% Cu","1ks",12.98937469150235,{"$f":"F12*(1-Elteq!$F$9)","v":12.98937469150235},"8591735031909"]
["TECHNIK","Cupal 50x 5",null,"Cupalový pásek 1,0x500x50mm, složení 70% Al + 30% Cu","1ks",15.587249629802821,{"$f":"F13*(1-Elteq!$F$9)","v":15.587249629802821},"8591735037543"]
["TECHNIK","Cupal 50x 6",null,"Cupalový pásek 1,0x500x60mm, složení 70% Al + 30% Cu","1ks",17.62843708132462,{"$f":"F14*(1-Elteq!$F$9)","v":17.62843708132462},"8591735039981"]
["TECHNIK","Cupal 50x 6/0,5",null,"Cupalový pásek 0,5x500x60mm, složení 70% Al + 30% Cu","1ks",15.958374620988602,{"$f":"F15*(1-Elteq!$F$9)","v":15.958374620988602},"8591735037546"]
["TECHNIK","Cupal 50x 8",null,"Cupalový pásek 1,0x500x80mm, složení 70% Al + 30% Cu","1ks",20.597437010810872,{"$f":"F16*(1-Elteq!$F$9)","v":20.597437010810872},"8591735037062"]
["TECHNIK","Cupal 50x 8/0,5",null,"Cupalový pásek 0,5x500x80mm, složení 70% Al + 30% Cu","1ks",17.257312090138839,{"$f":"F17*(1-Elteq!$F$9)","v":17.257312090138839},"8591735047153"]
["TECHNIK","Cupal 50x10",null,"Cupalový pásek 1,0x500x100mm, složení 70% Al + 30% Cu","1ks",23.751999435890014,{"$f":"F18*(1-Elteq!$F$9)","v":23.751999435890014},"8591735031916"]
["TECHNIK","Cupal 50x10/0,5",null,"Cupalový pásek 0,5x500x100mm, složení 70% Al + 30% Cu","1ks",21.525249488775323,{"$f":"F19*(1-Elteq!$F$9)","v":21.525249488775323},"8591735046064"]
["TECHNIK","Cupal 50x100",null,"Cupalový pásek 1,0x500x1000mm, složení 70% Al + 30% Cu","1ks",175.91324582206042,{"$f":"F20*(1-Elteq!$F$9)","v":175.91324582206042},"8591735031855"]
["TECHNIK","Cupal 50x11",null,"Cupalový pásek 1,0x500x110mm, složení 70% Al + 30% Cu","1ks",26.164311878597594,{"$f":"F21*(1-Elteq!$F$9)","v":26.164311878597594},"8591735052188"]
["TECHNIK","Cupal 50x12",null,"Cupalový pásek 1,0x500x120mm, složení 70% Al + 30% Cu","1ks",27.092124356562046,{"$f":"F22*(1-Elteq!$F$9)","v":27.092124356562046},"8591735036072"]
["TECHNIK","Cupal 50x17,5",null,"Cupalový pásek 1,0x500x175mm, složení 70% Al + 30% Cu","1ks",35.999124145020801,{"$f":"F23*(1-Elteq!$F$9)","v":35.999124145020801},"8591735054151"]
["TECHNIK","Cupal 50x20",null,"Cupalový pásek 1,0x500x200mm, složení 70% Al + 30% Cu","1ks",40.823749030435962,{"$f":"F24*(1-Elteq!$F$9)","v":40.823749030435962},"8591735031923"]
["TECHNIK","Cupal 50x25",null,"Cupalový pásek 1,0x500x250mm, složení 70% Al + 30% Cu","1ks",50.472998801266279,{"$f":"F25*(1-Elteq!$F$9)","v":50.472998801266279},"8591735053086"]
["TECHNIK","Cupal 50x30",null,"Cupalový pásek 1,0x500x300mm, složení 70% Al + 30% Cu","1ks",57.709936129389014,{"$f":"F26*(1-Elteq!$F$9)","v":57.709936129389014},"8591735031930"]
["TECHNIK","Cupal 50x50",null,"Cupalový pásek 1,0x500x500mm, složení 70% Al + 30% Cu","1ks",87.585497919844428,{"$f":"F27*(1-Elteq!$F$9)","v":87.585497919844428},"8591735052225"]
["TECHNIK","Cupal 50x50/0,5",null,"Cupalový pásek 0,5x500x500mm, složení 70% Al + 30% Cu","1ks",44.534998942293775,{"$f":"F28*(1-Elteq!$F$9)","v":44.534998942293775},""]
["TECHNIK","Cupal M 3",null,"Cupalová podložka pro svorník M3, síla 1mm, vnější ø 7,0mm / vnitřní ø 3,2mm","100ks",8.9069997884587551,{"$f":"F29*(1-Elteq!$F$9)","v":8.9069997884587551},"8591735034023"]
["TECHNIK","Cupal M 4",null,"Cupalová podložka pro svorník M4, síla 1mm, vnější ø 8,5mm / vnitřní ø 4,2mm","100ks",9.2781247796445356,{"$f":"F30*(1-Elteq!$F$9)","v":9.2781247796445356},"8591735029296"]
["TECHNIK","Cupal M 5",null,"Cupalová podložka pro svorník M5, síla 1mm, vnější ø 11,2mm / vnitřní ø 5,2mm","100ks",9.649249770830318,{"$f":"F31*(1-Elteq!$F$9)","v":9.649249770830318},"8591735019341"]
["TECHNIK","Cupal M 5/2",null,"Cupalová podložka pro svorník M5, síla 2mm","50ks",7.7936248149014107,{"$f":"F32*(1-Elteq!$F$9)","v":7.7936248149014107},"8591735048303"]
["TECHNIK","Cupal M 6",null,"Cupalová podložka pro svorník M6, síla 1mm, vnější ø 13,2mm / vnitřní ø 6,5mm","100ks",10.391499753201881,{"$f":"F33*(1-Elteq!$F$9)","v":10.391499753201881},"8591735009335"]
["TECHNIK","Cupal M 6/2",null,"Cupalová podložka pro svorník M6, síla 2mm","50ks",7.979187310494301,{"$f":"F34*(1-Elteq!$F$9)","v":7.979187310494301},"8591735048297"]
["TECHNIK","Cupal M 8",null,"Cupalová podložka pro svorník M8, síla 1mm, vnější ø 17,2mm / vnitřní ø 8,5mm","100ks",14.473874656245476,{"$f":"F35*(1-Elteq!$F$9)","v":14.473874656245476},"8591735009298"]
["TECHNIK","Cupal M 8/2",null,"Cupalová podložka pro svorník M8, síla 2mm","50ks",14.473874656245476,{"$f":"F36*(1-Elteq!$F$9)","v":14.473874656245476},"8591735048280"]
["TECHNIK","Cupal M10",null,"Cupalová podložka pro svorník M10, síla 1mm, vnější ø 21,2mm / vnitřní ø 11,0mm","100ks",21.154124497589542,{"$f":"F37*(1-Elteq!$F$9)","v":21.154124497589542},"8591735009304"]
["TECHNIK","Cupal M10/2",null,"Cupalová podložka pro svorník M10, síla 2mm","50ks",18.407799562814759,{"$f":"F38*(1-Elteq!$F$9)","v":18.407799562814759},"8591735047672"]
["TECHNIK","Cupal M12",null,"Cupalová podložka pro svorník M12, síla 1mm, vnější ø 28,2mm / vnitřní ø 13,0mm","50ks",16.329499612174384,{"$f":"F39*(1-Elteq!$F$9)","v":16.329499612174384},"8591735009311"]
["TECHNIK","Cupal M12/2",null,"Cupalová podložka pro svorník M12, síla 2mm","50ks",29.133311808083846,{"$f":"F40*(1-Elteq!$F$9)","v":29.133311808083846},"8591735048273"]
["TECHNIK","Cupal M14",null,"Cupalová podložka pro svorník M14, síla 1mm, vnější ø 32,0mm / vnitřní ø 15,0mm","50ks",25.60762439181892,{"$f":"F41*(1-Elteq!$F$9)","v":25.60762439181892},"8591735018108"]
["TECHNIK","Cupal M14/2",null,"Cupalová podložka pro svorník M14, síla 2mm","50ks",38.040311596542601,{"$f":"F42*(1-Elteq!$F$9)","v":38.040311596542601},"8591735048259"]
["TECHNIK","Cupal M16",null,"Cupalová podložka pro svorník M16, síla 1mm, vnější ø 35,0mm / vnitřní ø 17,0mm","50ks",24.494249418261575,{"$f":"F43*(1-Elteq!$F$9)","v":24.494249418261575},"8591735009328"]
["TECHNIK","Cupal M16/2",null,"Cupalová podložka pro svorník M16, síla 2mm","50ks",43.050498977550646,{"$f":"F44*(1-Elteq!$F$9)","v":43.050498977550646},"8591735048266"]
["TECHNIK","Cupal M20",null,"Cupalová podložka pro svorník M20, síla 1mm, vnější ø 40,0mm / vnitřní ø 21,0mm","50ks",32.287874233162988,{"$f":"F45*(1-Elteq!$F$9)","v":32.287874233162988},"8591735031848"]
["TECHNIK","Cupal M20/2",null,"Cupalová podložka pro svorník M20, síla 2mm","50ks",52.514186252788079,{"$f":"F46*(1-Elteq!$F$9)","v":52.514186252788079},"8591735048099"]
["TECHNIK","DD  0,25-8 fialová",null,"Dutinka dvojitá, průřez 2x0,25mm2 / délka 8mm, dle DIN46228, barva fialová","500ks",11.319312231166334,{"$f":"F47*(1-Elteq!$F$9)","v":11.319312231166334},"8591735014575"]
["TECHNIK","DD  0,25-8 modrá",null,"Dutinka dvojitá, průřez 2x0,25mm2 / délka 8mm, dle DIN46228, barva modrá","500ks",11.319312231166334,{"$f":"F48*(1-Elteq!$F$9)","v":11.319312231166334},"8591735014568"]
["TECHNIK","DD  0,25-8 modrá 100",null,"Dutinka dvojitá, průřez 2x0,25mm2 / délka 8mm, dle DIN46228, barva modrá (100ks)","100ks",2.820549933011939,{"$f":"F49*(1-Elteq!$F$9)","v":2.820549933011939},"8591735030377"]
["TECHNIK","DD  0,34-8 tyrkys100",null,"Dutinka dvojitá, průřez 2x0,34mm2 / délka 8mm, dle DIN46228, barva tyrkysová (100ks)","100ks",2.820549933011939,{"$f":"F50*(1-Elteq!$F$9)","v":2.820549933011939},"8591735030384"]
["TECHNIK","DD  0,34-8 tyrkysová",null,"Dutinka dvojitá, průřez 2x0,34mm2 / délka 8mm, dle DIN46228, barva tyrkysová","500ks",11.319312231166334,{"$f":"F51*(1-Elteq!$F$9)","v":11.319312231166334},"8591735014582"]
["TECHNIK","DD  0,5- 6 bílá",null,"Dutinka dvojitá, průřez 2x0,50mm2 / délka 6mm, dle DIN46228, barva bílá","500ks",11.319312231166334,{"$f":"F52*(1-Elteq!$F$9)","v":11.319312231166334},"8591735021863"]
["TECHNIK","DD  0,5- 6 oranž 100",null,"Dutinka dvojitá, průřez 2x0,50mm2 / délka 6mm, dle DIN46228, barva oranžová (100ks)","100ks",2.7463249347747829,{"$f":"F53*(1-Elteq!$F$9)","v":2.7463249347747829},"8591735030391"]
["TECHNIK","DD  0,5- 6 oranžová",null,"Dutinka dvojitá, průřez 2x0,50mm2 / délka 6mm, dle DIN46228, barva oranžová","500ks",11.319312231166334,{"$f":"F54*(1-Elteq!$F$9)","v":11.319312231166334},"8591735021856"]
["TECHNIK","DD  0,5- 8 bílá",null,"Dutinka dvojitá, průřez 2x0,50mm2 / délka 8mm, dle DIN46228, barva bílá","500ks",10.762624744387661,{"$f":"F55*(1-Elteq!$F$9)","v":10.762624744387661},"8591735000844"]
["TECHNIK","DD  0,5- 8 bílá 100",null,"Dutinka dvojitá, průřez 2x0,50mm2 / délka 8mm, dle DIN46228, barva bílá (100ks)","100ks",2.4494249418261576,{"$f":"F56*(1-Elteq!$F$9)","v":2.4494249418261576},"8591735030407"]
["TECHNIK","DD  0,5- 8 oranž 100",null,"Dutinka dvojitá, průřez 2x0,50mm2 / délka 8mm, dle DIN46228, barva oranžová (100ks)","100ks",2.4494249418261576,{"$f":"F57*(1-Elteq!$F$9)","v":2.4494249418261576},"8591735017521"]
["TECHNIK","DD  0,5- 8 oranžová",null,"Dutinka dvojitá, průřez 2x0,50mm2 / délka 8mm, dle DIN46228, barva oranžová","500ks",10.762624744387661,{"$f":"F58*(1-Elteq!$F$9)","v":10.762624744387661},"8591735000851"]
["TECHNIK","DD  0,5-10 bílá",null,"Dutinka dvojitá, průřez 2x0,50mm2 / délka 10mm, dle DIN46228, barva bílá","500ks",18.927374550474855,{"$f":"F59*(1-Elteq!$F$9)","v":18.927374550474855},"8591735014001"]
["TECHNIK","DD  0,5-10 bílá 100",null,"Dutinka dvojitá, průřez 2x0,50mm2 / délka 10mm, dle DIN46228, barva bílá (100ks)","100ks",4.2308248995179083,{"$f":"F60*(1-Elteq!$F$9)","v":4.2308248995179083},"8591735030414"]
["TECHNIK","DD  0,5-10 oranžová",null,"Dutinka dvojitá, průřez 2x0,50mm2 / délka 10mm, dle DIN46228, barva oranžová","500ks",18.927374550474855,{"$f":"F61*(1-Elteq!$F$9)","v":18.927374550474855},"8591735000868"]
["TECHNIK","DD  0,5-12 bílá",null,"Dutinka dvojitá, průřez 2x0,50mm2 / délka 12mm, dle DIN46228, barva bílá","500ks",30.246686781641188,{"$f":"F62*(1-Elteq!$F$9)","v":30.246686781641188},"8591735033699"]
["TECHNIK","DD  0,5-12 oranž 100",null,"Dutinka dvojitá, průřez 2x0,50mm2 / délka 12mm, dle DIN46228, barva oranžová (100ks)","100ks",7.19982482900416,{"$f":"F63*(1-Elteq!$F$9)","v":7.19982482900416},"8591735030421"]
["TECHNIK","DD  0,5-12 oranžová",null,"Dutinka dvojitá, průřez 2x0,50mm2 / délka 12mm, dle DIN46228, barva oranžová","500ks",30.246686781641188,{"$f":"F64*(1-Elteq!$F$9)","v":30.246686781641188},"8591735017262"]
["TECHNIK","DD  0,75- 8 bílá",null,"Dutinka dvojitá, průřez 2x0,75mm2 / délka 8mm, dle DIN46228, barva bílá","500ks",10.762624744387661,{"$f":"F65*(1-Elteq!$F$9)","v":10.762624744387661},"8591735000875"]
["TECHNIK","DD  0,75- 8 bílá 100",null,"Dutinka dvojitá, průřez 2x0,75mm2 / délka 8mm, dle DIN46228, barva bílá (100ks)","100ks",2.4494249418261576,{"$f":"F66*(1-Elteq!$F$9)","v":2.4494249418261576},"8591735017705"]
["TECHNIK","DD  0,75- 8 modrá",null,"Dutinka dvojitá, průřez 2x0,75mm2 / délka 8mm, dle DIN46228, barva modrá","500ks",10.762624744387661,{"$f":"F67*(1-Elteq!$F$9)","v":10.762624744387661},"8591735000882"]
["TECHNIK","DD  0,75- 8 modrá100",null,"Dutinka dvojitá, průřez 2x0,75mm2 / délka 8mm, dle DIN46228, barva modrá (100ks)","100ks",2.4494249418261576,{"$f":"F68*(1-Elteq!$F$9)","v":2.4494249418261576},"8591735047023"]
["TECHNIK","DD  0,75- 8 šedá",null,"Dutinka dvojitá, průřez 2x0,75mm2 / délka 8mm, dle DIN46228, barva šedá","500ks",10.762624744387661,{"$f":"F69*(1-Elteq!$F$9)","v":10.762624744387661},"8591735000899"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"DD  0,75- 8 šedá 100",null,"Dutinka dvojitá, průřez 2x0,75mm2 / délka 8mm, dle DIN46228, barva šedá (100ks)","100ks",2.4494249418261576,{"$f":"F70*(1-Elteq!$F$9)","v":2.4494249418261576},"8591735018344"]
["TECHNIK","DD  0,75-10 bílá",null,"Dutinka dvojitá, průřez 2x0,75mm2 / délka 10mm, dle DIN46228, barva bílá","500ks",19.112937046067746,{"$f":"F71*(1-Elteq!$F$9)","v":19.112937046067746},"8591735000905"]
["TECHNIK","DD  0,75-10 bílá 100",null,"Dutinka dvojitá, průřez 2x0,75mm2 / délka 10mm, dle DIN46228, barva bílá (100ks)","100ks",4.2308248995179083,{"$f":"F72*(1-Elteq!$F$9)","v":4.2308248995179083},"8591735018436"]
["TECHNIK","DD  0,75-10 modrá",null,"Dutinka dvojitá, průřez 2x0,75mm2 / délka 10mm, dle DIN46228, barva modrá","500ks",19.112937046067746,{"$f":"F73*(1-Elteq!$F$9)","v":19.112937046067746},"8591735000912"]
["TECHNIK","DD  0,75-10 šedá",null,"Dutinka dvojitá, průřez 2x0,75mm2 / délka 10mm, dle DIN46228, barva šedá","500ks",19.112937046067746,{"$f":"F74*(1-Elteq!$F$9)","v":19.112937046067746},"8591735000929"]
["TECHNIK","DD  0,75-12 bílá",null,"Dutinka dvojitá, průřez 2x0,75mm2 / délka 12mm, dle DIN46228, barva bílá","500ks",20.597437010810872,{"$f":"F75*(1-Elteq!$F$9)","v":20.597437010810872},"8591735029135"]
["TECHNIK","DD  0,75-12 bílá 100",null,"Dutinka dvojitá, průřez 2x0,75mm2 / délka 12mm, dle DIN46228, barva bílá (100ks)","100ks",4.7503998871780029,{"$f":"F76*(1-Elteq!$F$9)","v":4.7503998871780029},"8591735030438"]
["TECHNIK","DD  0,75-12 modrá",null,"Dutinka dvojitá, průřez 2x0,75mm2 / délka 12mm, dle DIN46228, barva modrá","500ks",20.597437010810872,{"$f":"F77*(1-Elteq!$F$9)","v":20.597437010810872},"8591735029142"]
["TECHNIK","DD  0,75-12 šedá",null,"Dutinka dvojitá, průřez 2x0,75mm2 / délka 12mm, dle DIN46228, barva šedá","500ks",20.597437010810872,{"$f":"F78*(1-Elteq!$F$9)","v":20.597437010810872},"8591735029159"]
["TECHNIK","DD  0,75-18 bílá",null,"Dutinka dvojitá, průřez 2x0,75mm2 / délka 18mm, dle DIN46228, barva bílá","500ks",30.246686781641188,{"$f":"F79*(1-Elteq!$F$9)","v":30.246686781641188},"8591735018481"]
["TECHNIK","DD  0,75-18 bílá 100",null,"Dutinka dvojitá, průřez 2x0,75mm2 / délka 18mm, dle DIN46228, barva bílá (100ks)","100ks",7.19982482900416,{"$f":"F80*(1-Elteq!$F$9)","v":7.19982482900416},"8591735030445"]
["TECHNIK","DD  1,0- 8 rudá",null,"Dutinka dvojitá, průřez 2x1,0mm2 / délka 8mm, dle DIN46228, barva rudá","500ks",10.762624744387661,{"$f":"F81*(1-Elteq!$F$9)","v":10.762624744387661},"8591735000936"]
["TECHNIK","DD  1,0- 8 rudá 100",null,"Dutinka dvojitá, průřez 2x1,0mm2 / délka 8mm, dle DIN46228, barva rudá (100ks)","100ks",2.4494249418261576,{"$f":"F82*(1-Elteq!$F$9)","v":2.4494249418261576},"8591735018887"]
["TECHNIK","DD  1,0- 8 žlutá",null,"Dutinka dvojitá, průřez 2x1,0mm2 / délka 8mm, dle DIN46228, barva žlutá","500ks",10.762624744387661,{"$f":"F83*(1-Elteq!$F$9)","v":10.762624744387661},"8591735000943"]
["TECHNIK","DD  1,0- 8 žlutá 100",null,"Dutinka dvojitá, průřez 2x1,0mm2 / délka 8mm, dle DIN46228, barva žlutá (100ks)","100ks",2.4494249418261576,{"$f":"F84*(1-Elteq!$F$9)","v":2.4494249418261576},"8591735017460"]
["TECHNIK","DD  1,0-10 rudá",null,"Dutinka dvojitá, průřez 2x1,0mm2 / délka 10mm, dle DIN46228, barva rudá","500ks",19.855187028439307,{"$f":"F85*(1-Elteq!$F$9)","v":19.855187028439307},"8591735000950"]
["TECHNIK","DD  1,0-10 rudá 100",null,"Dutinka dvojitá, průřez 2x1,0mm2 / délka 10mm, dle DIN46228, barva rudá (100ks)","100ks",4.2308248995179083,{"$f":"F86*(1-Elteq!$F$9)","v":4.2308248995179083},"8591735033323"]
["TECHNIK","DD  1,0-10 žlutá",null,"Dutinka dvojitá, průřez 2x1,0mm2 / délka 10mm, dle DIN46228, barva žlutá","500ks",19.855187028439307,{"$f":"F87*(1-Elteq!$F$9)","v":19.855187028439307},"8591735000967"]
["TECHNIK","DD  1,0-10 žlutá 100",null,"Dutinka dvojitá, průřez 2x1,0mm2 / délka 10mm, dle DIN46228, barva žlutá (100ks)","100ks",4.2308248995179083,{"$f":"F88*(1-Elteq!$F$9)","v":4.2308248995179083},"8591735017781"]
["TECHNIK","DD  1,0-12 rudá",null,"Dutinka dvojitá, průřez 2x1,0mm2 / délka 12mm, dle DIN46228, barva rudá","500ks",20.782999506403762,{"$f":"F89*(1-Elteq!$F$9)","v":20.782999506403762},"8591735020057"]
["TECHNIK","DD  1,0-12 rudá 100",null,"Dutinka dvojitá, průřez 2x1,0mm2 / délka 12mm, dle DIN46228, barva rudá (100ks)","100ks",4.7503998871780029,{"$f":"F90*(1-Elteq!$F$9)","v":4.7503998871780029},"8591735037031"]
["TECHNIK","DD  1,0-12 žlutá",null,"Dutinka dvojitá, průřez 2x1,0mm2 / délka 12mm, dle DIN46228, barva žlutá","500ks",20.782999506403762,{"$f":"F91*(1-Elteq!$F$9)","v":20.782999506403762},"8591735018498"]
["TECHNIK","DD  1,0-12 žlutá 100",null,"Dutinka dvojitá, průřez 2x1,0mm2 / délka 12mm, dle DIN46228, barva žlutá (100ks)","100ks",4.7503998871780029,{"$f":"F92*(1-Elteq!$F$9)","v":4.7503998871780029},"8591735018467"]
["TECHNIK","DD  1,0-18 rudá",null,"Dutinka dvojitá, průřez 2x1,0mm2 / délka 18mm, dle DIN46228, barva rudá","500ks",30.246686781641188,{"$f":"F93*(1-Elteq!$F$9)","v":30.246686781641188},"8591735017873"]
["TECHNIK","DD  1,0-18 žlutá",null,"Dutinka dvojitá, průřez 2x1,0mm2 / délka 18mm, dle DIN46228, barva žlutá","500ks",30.246686781641188,{"$f":"F94*(1-Elteq!$F$9)","v":30.246686781641188},"8591735017880"]
["TECHNIK","DD  1,0-18 žlutá 100",null,"Dutinka dvojitá, průřez 2x1,0mm2 / délka 18mm, dle DIN46228, barva žlutá (100ks)","100ks",7.19982482900416,{"$f":"F95*(1-Elteq!$F$9)","v":7.19982482900416},"8591735030452"]
["TECHNIK","DD  1,5- 8 černá",null,"Dutinka dvojitá, průřez 2x1,5mm2 / délka 8mm, dle DIN46228, barva černá","500ks",10.762624744387661,{"$f":"F96*(1-Elteq!$F$9)","v":10.762624744387661},"8591735000974"]
["TECHNIK","DD  1,5- 8 černá 100",null,"Dutinka dvojitá, průřez 2x1,5mm2 / délka 8mm, dle DIN46228, barva černá (100ks)","100ks",2.4494249418261576,{"$f":"F97*(1-Elteq!$F$9)","v":2.4494249418261576},"8591735030469"]
["TECHNIK","DD  1,5- 8 rudá",null,"Dutinka dvojitá, průřez 2x1,5mm2 / délka 8mm, dle DIN46228, barva rudá","500ks",10.762624744387661,{"$f":"F98*(1-Elteq!$F$9)","v":10.762624744387661},"8591735000981"]
["TECHNIK","DD  1,5- 8 rudá 100",null,"Dutinka dvojitá, průřez 2x1,5mm2 / délka 8mm, dle DIN46228, barva rudá (100ks)","100ks",2.4494249418261576,{"$f":"F99*(1-Elteq!$F$9)","v":2.4494249418261576},"8591735017453"]
["TECHNIK","DD  1,5-12 černá",null,"Dutinka dvojitá, průřez 2x1,5mm2 / délka 12mm, dle DIN46228, barva černá","500ks",19.855187028439307,{"$f":"F100*(1-Elteq!$F$9)","v":19.855187028439307},"8591735000998"]
["TECHNIK","DD  1,5-12 černá 100",null,"Dutinka dvojitá, průřez 2x1,5mm2 / délka 12mm, dle DIN46228, barva černá (100ks)","100ks",4.4163873951107995,{"$f":"F101*(1-Elteq!$F$9)","v":4.4163873951107995},"8591735033330"]
["TECHNIK","DD  1,5-12 rudá",null,"Dutinka dvojitá, průřez 2x1,5mm2 / délka 12mm, dle DIN46228, barva rudá","500ks",19.855187028439307,{"$f":"F102*(1-Elteq!$F$9)","v":19.855187028439307},"8591735001001"]
["TECHNIK","DD  1,5-12 rudá 100",null,"Dutinka dvojitá, průřez 2x1,5mm2 / délka 12mm, dle DIN46228, barva rudá (100ks)","100ks",4.4163873951107995,{"$f":"F103*(1-Elteq!$F$9)","v":4.4163873951107995},"8591735018443"]
["TECHNIK","DD  1,5-18 černá",null,"Dutinka dvojitá, průřez 2x1,5mm2 / délka 18mm, dle DIN46228, barva černá","100ks",7.19982482900416,{"$f":"F104*(1-Elteq!$F$9)","v":7.19982482900416},"8591735048884"]
["TECHNIK","DD  1,5-18 rudá",null,"Dutinka dvojitá, průřez 2x1,5mm2 / délka 18mm, dle DIN46228, barva rudá","100ks",7.19982482900416,{"$f":"F105*(1-Elteq!$F$9)","v":7.19982482900416},"8591735016326"]
["TECHNIK","DD  2,5-10 modrá",null,"Dutinka dvojitá, průřez 2x2,5mm2 / délka 10mm, dle DIN46228, barva modrá","250ks",6.1235623545653937,{"$f":"F106*(1-Elteq!$F$9)","v":6.1235623545653937},"8591735001018"]
["TECHNIK","DD  2,5-10 modrá 100",null,"Dutinka dvojitá, průřez 2x2,5mm2 / délka 10mm, dle DIN46228, barva modrá (100ks)","100ks",2.7463249347747829,{"$f":"F107*(1-Elteq!$F$9)","v":2.7463249347747829},"8591735030162"]
["TECHNIK","DD  2,5-10 šedá",null,"Dutinka dvojitá, průřez 2x2,5mm2 / délka 10mm, dle DIN46228, barva šedá","250ks",6.1235623545653937,{"$f":"F108*(1-Elteq!$F$9)","v":6.1235623545653937},"8591735001025"]
["TECHNIK","DD  2,5-10 šedá 100",null,"Dutinka dvojitá, průřez 2x2,5mm2 / délka 10mm, dle DIN46228, barva šedá (100ks)","100ks",2.7463249347747829,{"$f":"F109*(1-Elteq!$F$9)","v":2.7463249347747829},"8591735036454"]
["TECHNIK","DD  2,5-13 modrá",null,"Dutinka dvojitá, průřez 2x2,5mm2 / délka 13mm, dle DIN46228, barva modrá","250ks",11.319312231166334,{"$f":"F110*(1-Elteq!$F$9)","v":11.319312231166334},"8591735001032"]
["TECHNIK","DD  2,5-13 modrá 100",null,"Dutinka dvojitá, průřez 2x2,5mm2 / délka 13mm, dle DIN46228, barva modrá (100ks)","100ks",5.0101873810080493,{"$f":"F111*(1-Elteq!$F$9)","v":5.0101873810080493},"8591735018450"]
["TECHNIK","DD  2,5-13 šedá",null,"Dutinka dvojitá, průřez 2x2,5mm2 / délka 13mm, dle DIN46228, barva šedá","250ks",11.319312231166334,{"$f":"F112*(1-Elteq!$F$9)","v":11.319312231166334},"8591735001049"]
["TECHNIK","DD  2,5-18 modrá",null,"Dutinka dvojitá, průřez 2x2,5mm2 / délka 18mm, dle DIN46228, barva modrá","100ks",7.7565123157828326,{"$f":"F113*(1-Elteq!$F$9)","v":7.7565123157828326},"8591735018504"]
["TECHNIK","DD  2,5-18 šedá",null,"Dutinka dvojitá, průřez 2x2,5mm2 / délka 18mm, dle DIN46228, barva šedá","100ks",7.7565123157828326,{"$f":"F114*(1-Elteq!$F$9)","v":7.7565123157828326},"8591735027889"]
["TECHNIK","DD  4-12 oranžová",null,"Dutinka dvojitá, průřez 2x4,0mm2 / délka 12mm, dle DIN46228, barva oranžová","100ks",8.2018623052057702,{"$f":"F115*(1-Elteq!$F$9)","v":8.2018623052057702},"8591735001056"]
["TECHNIK","DD  4-12 šedá",null,"Dutinka dvojitá, průřez 2x4,0mm2 / délka 12mm, dle DIN46228, barva šedá","100ks",8.2018623052057702,{"$f":"F116*(1-Elteq!$F$9)","v":8.2018623052057702},"8591735001063"]
["TECHNIK","DD  4-18 šedá",null,"Dutinka dvojitá, průřez 2x4,0mm2 / délka 18mm, dle DIN46228, barva šedá","100ks",14.62232465271979,{"$f":"F117*(1-Elteq!$F$9)","v":14.62232465271979},"8591735001070"]
["TECHNIK","DD  6-14 černá",null,"Dutinka dvojitá, průřez 2x6,0mm2 / délka 14mm, dle DIN46228, barva černá","100ks",10.465724751439037,{"$f":"F118*(1-Elteq!$F$9)","v":10.465724751439037},"8591735001087"]
["TECHNIK","DD  6-14 zelená",null,"Dutinka dvojitá, průřez 2x6,0mm2 / délka 14mm, dle DIN46228, barva zelená","100ks",10.465724751439037,{"$f":"F119*(1-Elteq!$F$9)","v":10.465724751439037},"8591735001094"]
["TECHNIK","DD  6-14 žlutá",null,"Dutinka dvojitá, průřez 2x6,0mm2 / délka 14mm, dle DIN46228, barva žlutá","100ks",10.465724751439037,{"$f":"F120*(1-Elteq!$F$9)","v":10.465724751439037},"8591735001100"]
["TECHNIK","DD  6-18 černá",null,"Dutinka dvojitá, průřez 2x6,0mm2 / délka 18mm, dle DIN46228, barva černá","100ks",16.997524596308789,{"$f":"F121*(1-Elteq!$F$9)","v":16.997524596308789},"8591735001117"]
["TECHNIK","DD  6-18 žlutá",null,"Dutinka dvojitá, průřez 2x6,0mm2 / délka 18mm, dle DIN46228, barva žlutá","100ks",16.997524596308789,{"$f":"F122*(1-Elteq!$F$9)","v":16.997524596308789},"8591735013325"]
["TECHNIK","DD 10-14 hnědá",null,"Dutinka dvojitá, průřez 2x10mm2 / délka 14mm, dle DIN46228, barva hnědá","100ks",12.878037194146616,{"$f":"F123*(1-Elteq!$F$9)","v":12.878037194146616},"8591735029371"]
["TECHNIK","DD 10-14 rudá",null,"Dutinka dvojitá, průřez 2x10mm2 / délka 14mm, dle DIN46228, barva rudá","100ks",12.878037194146616,{"$f":"F124*(1-Elteq!$F$9)","v":12.878037194146616},"8591735001131"]
["TECHNIK","DD 10-14 sl. kost",null,"Dutinka dvojitá, průřez 2x10mm2 / délka 14mm, dle DIN46228, barva sl. kost","100ks",12.878037194146616,{"$f":"F125*(1-Elteq!$F$9)","v":12.878037194146616},"8591735001124"]
["TECHNIK","DD 10-18 sl. kost",null,"Dutinka dvojitá, průřez 2x10mm2 / délka 18mm, dle DIN46228, barva sl. kost","100ks",19.59539953460926,{"$f":"F126*(1-Elteq!$F$9)","v":19.59539953460926},"8591735009724"]
["TECHNIK","DD 16-14 bílá",null,"Dutinka dvojitá, průřez 2x16mm2 / délka 14mm, dle DIN46228, barva bílá","50ks",9.3894622770002716,{"$f":"F127*(1-Elteq!$F$9)","v":9.3894622770002716},"8591735018511"]
["TECHNIK","DD 16-14 modrá",null,"Dutinka dvojitá, průřez 2x16mm2 / délka 14mm, dle DIN46228, barva modrá","50ks",9.3894622770002716,{"$f":"F128*(1-Elteq!$F$9)","v":9.3894622770002716},"8591735001148"]
["TECHNIK","DD 16-14 zelená",null,"Dutinka dvojitá, průřez 2x16mm2 / délka 14mm, dle DIN46228, barva zelená","50ks",9.3894622770002716,{"$f":"F129*(1-Elteq!$F$9)","v":9.3894622770002716},"8591735001155"]
["TECHNIK","DD 16-16 zelená",null,"Dutinka dvojitá, průřez 2x16mm2 / délka 16mm, dle DIN46228, barva zelená","50ks",9.7234747690674741,{"$f":"F130*(1-Elteq!$F$9)","v":9.7234747690674741},"8591735021344"]
["TECHNIK","DD 16-25 zelená",null,"Dutinka dvojitá, průřez 2x16mm2 / délka 25mm, dle DIN46228, barva zelená","50ks",14.659437151838368,{"$f":"F131*(1-Elteq!$F$9)","v":14.659437151838368},"8591735009731"]
["TECHNIK","DI  0,14- 6 hnědá",null,"Dutinka izolovaná, průřez 0,14mm2 / délka 6mm, dle DIN46228, barva hnědá","500ks",9.3523497778816935,{"$f":"F132*(1-Elteq!$F$9)","v":9.3523497778816935},"8591735000011"]
["TECHNIK","DI  0,14- 6 hnědá100",null,"Dutinka izolovaná, průřez 0,14mm2 / délka 6mm, dle DIN46228, barva hnědá (100ks)","100ks",2.1525249488775327,{"$f":"F133*(1-Elteq!$F$9)","v":2.1525249488775327},"8591735038694"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"DI  0,14- 6 šedá",null,"Dutinka izolovaná, průřez 0,14mm2 / délka 6mm, dle DIN46228, barva šedá","500ks",9.3523497778816935,{"$f":"F134*(1-Elteq!$F$9)","v":9.3523497778816935},"8591735000028"]
["TECHNIK","DI  0,14- 6 šedá 100",null,"Dutinka izolovaná, průřez 0,14mm2 / délka 6mm, dle DIN46228, barva šedá (100ks)","100ks",2.1525249488775327,{"$f":"F135*(1-Elteq!$F$9)","v":2.1525249488775327},"8591735030193"]
["TECHNIK","DI  0,14- 8 hnědá",null,"Dutinka izolovaná, průřez 0,14mm2 / délka 8mm, dle DIN46228, barva hnědá","500ks",9.7605872681860522,{"$f":"F136*(1-Elteq!$F$9)","v":9.7605872681860522},"8591735000035"]
["TECHNIK","DI  0,14- 8 hnědá100",null,"Dutinka izolovaná, průřez 0,14mm2 / délka 8mm, dle DIN46228, barva hnědá (100ks)","100ks",2.3009749453518449,{"$f":"F137*(1-Elteq!$F$9)","v":2.3009749453518449},"8591735038908"]
["TECHNIK","DI  0,14- 8 šedá",null,"Dutinka izolovaná, průřez 0,14mm2 / délka 8mm, dle DIN46228, barva šedá","500ks",9.7605872681860522,{"$f":"F138*(1-Elteq!$F$9)","v":9.7605872681860522},"8591735000042"]
["TECHNIK","DI  0,14- 8 šedá 100",null,"Dutinka izolovaná, průřez 0,14mm2 / délka 8mm, dle DIN46228, barva šedá (100ks)","100ks",2.3009749453518449,{"$f":"F139*(1-Elteq!$F$9)","v":2.3009749453518449},"8591735030209"]
["TECHNIK","DI  0,25- 6 fialová",null,"Dutinka izolovaná, průřez 0,25mm2 / délka 6mm, dle DIN46228, barva fialová","500ks",9.3523497778816935,{"$f":"F140*(1-Elteq!$F$9)","v":9.3523497778816935},"8591735056124"]
["TECHNIK","DI  0,25- 6 modrá",null,"Dutinka izolovaná, průřez 0,25mm2 / délka 6mm, dle DIN46228, barva modrá","500ks",9.3523497778816935,{"$f":"F141*(1-Elteq!$F$9)","v":9.3523497778816935},"8591735000059"]
["TECHNIK","DI  0,25- 6 modrá100",null,"Dutinka izolovaná, průřez 0,25mm2 / délka 6mm, dle DIN46228, barva modrá (100ks)","100ks",2.1525249488775327,{"$f":"F142*(1-Elteq!$F$9)","v":2.1525249488775327},"8591735030216"]
["TECHNIK","DI  0,25- 6 žlutá",null,"Dutinka izolovaná, průřez 0,25mm2 / délka 6mm, dle DIN46228, barva žlutá","500ks",9.3523497778816935,{"$f":"F143*(1-Elteq!$F$9)","v":9.3523497778816935},"8591735021085"]
["TECHNIK","DI  0,25- 8 fial.100",null,"Dutinka izolovaná, průřez 0,25mm2 / délka 8mm, dle DIN46228, barva fialová (100ks)","100ks",2.3009749453518449,{"$f":"F144*(1-Elteq!$F$9)","v":2.3009749453518449},"8591735033514"]
["TECHNIK","DI  0,25- 8 fialová",null,"Dutinka izolovaná, průřez 0,25mm2 / délka 8mm, dle DIN46228, barva fialová","500ks",10.391499753201881,{"$f":"F145*(1-Elteq!$F$9)","v":10.391499753201881},"8591735010812"]
["TECHNIK","DI  0,25- 8 modrá",null,"Dutinka izolovaná, průřez 0,25mm2 / délka 8mm, dle DIN46228, barva modrá","500ks",10.391499753201881,{"$f":"F146*(1-Elteq!$F$9)","v":10.391499753201881},"8591735000066"]
["TECHNIK","DI  0,25- 8 modrá100",null,"Dutinka izolovaná, průřez 0,25mm2 / délka 8mm, dle DIN46228, barva modrá (100ks)","100ks",2.3009749453518449,{"$f":"F147*(1-Elteq!$F$9)","v":2.3009749453518449},"8591735018979"]
["TECHNIK","DI  0,25- 8 žlutá",null,"Dutinka izolovaná, průřez 0,25mm2 / délka 8mm, dle DIN46228, barva žlutá","500ks",10.391499753201881,{"$f":"F148*(1-Elteq!$F$9)","v":10.391499753201881},"8591735021092"]
["TECHNIK","DI  0,25- 8 žlutá100",null,"Dutinka izolovaná, průřez 0,25mm2 / délka 8mm, dle DIN46228, barva žlutá (100ks)","100ks",2.3009749453518449,{"$f":"F149*(1-Elteq!$F$9)","v":2.3009749453518449},"8591735056360"]
["TECHNIK","DI  0,25-12 fialová",null,"Dutinka izolovaná, průřez 0,25mm2 / délka 12mm, dle DIN46228, barva fialová","500ks",16.40372461041154,{"$f":"F150*(1-Elteq!$F$9)","v":16.40372461041154},"8591735041328"]
["TECHNIK","DI  0,25-12 modrá",null,"Dutinka izolovaná, průřez 0,25mm2 / délka 12mm, dle DIN46228, barva modrá","500ks",16.40372461041154,{"$f":"F151*(1-Elteq!$F$9)","v":16.40372461041154},"8591735041335"]
["TECHNIK","DI  0,34- 6 růžová",null,"Dutinka izolovaná, průřez 0,34mm2 / délka 6mm, dle DIN46228, barva růžová","500ks",9.3523497778816935,{"$f":"F152*(1-Elteq!$F$9)","v":9.3523497778816935},"8591735047474"]
["TECHNIK","DI  0,34- 6 tyrk 100",null,"Dutinka izolovaná, průřez 0,34mm2 / délka 6mm, dle DIN46228, barva tyrkysová (100ks)","100ks",2.1525249488775327,{"$f":"F153*(1-Elteq!$F$9)","v":2.1525249488775327},"8591735030223"]
["TECHNIK","DI  0,34- 6 tyrkys.",null,"Dutinka izolovaná, průřez 0,34mm2 / délka 6mm, dle DIN46228, barva tyrkysová","500ks",9.3523497778816935,{"$f":"F154*(1-Elteq!$F$9)","v":9.3523497778816935},"8591735000073"]
["TECHNIK","DI  0,34- 6 zelená",null,"Dutinka izolovaná, průřez 0,34mm2 / délka 6mm, dle DIN46228, barva zelená","500ks",9.3523497778816935,{"$f":"F155*(1-Elteq!$F$9)","v":9.3523497778816935},"8591735047498"]
["TECHNIK","DI  0,34- 6 žlutá",null,"Dutinka izolovaná, průřez 0,34mm2 / délka 6mm, dle DIN46228, barva žlutá","500ks",9.3523497778816935,{"$f":"F156*(1-Elteq!$F$9)","v":9.3523497778816935},"8591735047481"]
["TECHNIK","DI  0,34- 8 růžo 100",null,"Dutinka izolovaná, průřez 0,34mm2 / délka 8mm, dle DIN46228, barva růžová (100ks)","100ks",2.3009749453518449,{"$f":"F157*(1-Elteq!$F$9)","v":2.3009749453518449},"8591735056476"]
["TECHNIK","DI  0,34- 8 růžová",null,"Dutinka izolovaná, průřez 0,34mm2 / délka 8mm, dle DIN46228, barva růžová","500ks",10.391499753201881,{"$f":"F158*(1-Elteq!$F$9)","v":10.391499753201881},"8591735047504"]
["TECHNIK","DI  0,34- 8 tyrk 100",null,"Dutinka izolovaná, průřez 0,34mm2 / délka 8mm, dle DIN46228, barva tyrkysová (100ks)","100ks",2.3009749453518449,{"$f":"F159*(1-Elteq!$F$9)","v":2.3009749453518449},"8591735030230"]
["TECHNIK","DI  0,34- 8 tyrkys.",null,"Dutinka izolovaná, průřez 0,34mm2 / délka 8mm, dle DIN46228, barva tyrkysová","500ks",10.391499753201881,{"$f":"F160*(1-Elteq!$F$9)","v":10.391499753201881},"8591735000080"]
["TECHNIK","DI  0,34- 8 zele 100",null,"Dutinka izolovaná, průřez 0,34mm2 / délka 8mm, dle DIN46228, barva zelená (100ks)","100ks",2.3009749453518449,{"$f":"F161*(1-Elteq!$F$9)","v":2.3009749453518449},"8591735056841"]
["TECHNIK","DI  0,34- 8 zelená",null,"Dutinka izolovaná, průřez 0,34mm2 / délka 8mm, dle DIN46228, barva zelená","500ks",10.391499753201881,{"$f":"F162*(1-Elteq!$F$9)","v":10.391499753201881},"8591735047511"]
["TECHNIK","DI  0,34- 8 žlutá",null,"Dutinka izolovaná, průřez 0,34mm2 / délka 8mm, dle DIN46228, barva žlutá","500ks",10.391499753201881,{"$f":"F163*(1-Elteq!$F$9)","v":10.391499753201881},"8591735047528"]
["TECHNIK","DI  0,34-12 růžová",null,"Dutinka izolovaná, průřez 0,34mm2 / délka 12mm, dle DIN46228, barva růžová","500ks",16.40372461041154,{"$f":"F164*(1-Elteq!$F$9)","v":16.40372461041154},"8591735041359"]
["TECHNIK","DI  0,34-12 tyrkys.",null,"Dutinka izolovaná, průřez 0,34mm2 / délka 12mm, dle DIN46228, barva tyrkysová","500ks",16.40372461041154,{"$f":"F165*(1-Elteq!$F$9)","v":16.40372461041154},"8591735041342"]
["TECHNIK","DI  0,5- 6 bílá",null,"Dutinka izolovaná, průřez 0,50mm2 / délka 6mm, dle DIN46228, barva bílá","500ks",6.6802498413440663,{"$f":"F166*(1-Elteq!$F$9)","v":6.6802498413440663},"8591735000097"]
["TECHNIK","DI  0,5- 6 bílá 100",null,"Dutinka izolovaná, průřez 0,50mm2 / délka 6mm, dle DIN46228, barva bílá (100ks)","100ks",1.4844999647431258,{"$f":"F167*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735030247"]
["TECHNIK","DI  0,5- 6 oranž 100",null,"Dutinka izolovaná, průřez 0,50mm2 / délka 6mm, dle DIN46228, barva oranžová (100ks)","100ks",1.4844999647431258,{"$f":"F168*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735030254"]
["TECHNIK","DI  0,5- 6 oranžová",null,"Dutinka izolovaná, průřez 0,50mm2 / délka 6mm, dle DIN46228, barva oranžová","500ks",6.6802498413440663,{"$f":"F169*(1-Elteq!$F$9)","v":6.6802498413440663},"8591735000103"]
["TECHNIK","DI  0,5- 8 bílá",null,"Dutinka izolovaná, průřez 0,50mm2 / délka 8mm, dle DIN46228, barva bílá","500ks",4.0823749030435961,{"$f":"F170*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735000110"]
["TECHNIK","DI  0,5- 8 bílá 100",null,"Dutinka izolovaná, průřez 0,50mm2 / délka 8mm, dle DIN46228, barva bílá (100ks)","100ks",0.89069997884587548,{"$f":"F171*(1-Elteq!$F$9)","v":0.89069997884587548},"8591735018122"]
["TECHNIK","DI  0,5- 8 oranž 100",null,"Dutinka izolovaná, průřez 0,50mm2 / délka 8mm, dle DIN46228, barva oranžová (100ks)","100ks",0.89069997884587548,{"$f":"F172*(1-Elteq!$F$9)","v":0.89069997884587548},"8591735017729"]
["TECHNIK","DI  0,5- 8 oranžová",null,"Dutinka izolovaná, průřez 0,50mm2 / délka 8mm, dle DIN46228, barva oranžová","500ks",4.0823749030435961,{"$f":"F173*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735000127"]
["TECHNIK","DI  0,5-10 bílá",null,"Dutinka izolovaná, průřez 0,50mm2 / délka 10mm, dle DIN46228, barva bílá","500ks",8.3503123016800824,{"$f":"F174*(1-Elteq!$F$9)","v":8.3503123016800824},"8591735000134"]
["TECHNIK","DI  0,5-10 bílá 100",null,"Dutinka izolovaná, průřez 0,50mm2 / délka 10mm, dle DIN46228, barva bílá (100ks)","100ks",1.781399957691751,{"$f":"F175*(1-Elteq!$F$9)","v":1.781399957691751},"8591735018269"]
["TECHNIK","DI  0,5-10 oranž 100",null,"Dutinka izolovaná, průřez 0,50mm2 / délka 10mm, dle DIN46228, barva oranžová (100ks)","100ks",1.781399957691751,{"$f":"F176*(1-Elteq!$F$9)","v":1.781399957691751},"8591735030261"]
["TECHNIK","DI  0,5-10 oranžová",null,"Dutinka izolovaná, průřez 0,50mm2 / délka 10mm, dle DIN46228, barva oranžová","500ks",8.3503123016800824,{"$f":"F177*(1-Elteq!$F$9)","v":8.3503123016800824},"8591735000141"]
["TECHNIK","DI  0,5-12 bílá",null,"Dutinka izolovaná, průřez 0,50mm2 / délka 12mm, dle DIN46228, barva bílá","500ks",10.205937257608991,{"$f":"F178*(1-Elteq!$F$9)","v":10.205937257608991},"8591735046385"]
["TECHNIK","DI  0,5-12 oranž 100",null,"Dutinka izolovaná, průřez 0,50mm2 / délka 12mm, dle DIN46228, barva oranžová (100ks)","100ks",2.2267499471146888,{"$f":"F179*(1-Elteq!$F$9)","v":2.2267499471146888},"8591735052782"]
["TECHNIK","DI  0,5-12 oranžová",null,"Dutinka izolovaná, průřez 0,50mm2 / délka 12mm, dle DIN46228, barva oranžová","500ks",10.205937257608991,{"$f":"F180*(1-Elteq!$F$9)","v":10.205937257608991},"8591735030698"]
["TECHNIK","DI  0,75- 6 bílá",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 6mm, dle DIN46228, barva bílá","500ks",6.6802498413440663,{"$f":"F181*(1-Elteq!$F$9)","v":6.6802498413440663},"8591735000158"]
["TECHNIK","DI  0,75- 6 bílá 100",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 6mm, dle DIN46228, barva bílá (100ks)","100ks",1.4844999647431258,{"$f":"F182*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735030278"]
["TECHNIK","DI  0,75- 6 modrá",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 6mm, dle DIN46228, barva modrá","500ks",6.6802498413440663,{"$f":"F183*(1-Elteq!$F$9)","v":6.6802498413440663},"8591735004910"]
["TECHNIK","DI  0,75- 6 šedá",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 6mm, dle DIN46228, barva šedá","500ks",6.6802498413440663,{"$f":"F184*(1-Elteq!$F$9)","v":6.6802498413440663},"8591735000165"]
["TECHNIK","DI  0,75- 6 šedá 100",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 6mm, dle DIN46228, barva šedá (100ks)","100ks",1.4844999647431258,{"$f":"F185*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735017392"]
["TECHNIK","DI  0,75- 8 bílá",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 8mm, dle DIN46228, barva bílá","500ks",4.0823749030435961,{"$f":"F186*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735000172"]
["TECHNIK","DI  0,75- 8 bílá 100",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 8mm, dle DIN46228, barva bílá (100ks)","100ks",0.89069997884587548,{"$f":"F187*(1-Elteq!$F$9)","v":0.89069997884587548},"8591735017538"]
["TECHNIK","DI  0,75- 8 modrá",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 8mm, dle DIN46228, barva modrá","500ks",4.0823749030435961,{"$f":"F188*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735000189"]
["TECHNIK","DI  0,75- 8 modrá100",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 8mm, dle DIN46228, barva modrá (100ks)","100ks",0.89069997884587548,{"$f":"F189*(1-Elteq!$F$9)","v":0.89069997884587548},"8591735017798"]
["TECHNIK","DI  0,75- 8 šedá",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 8mm, dle DIN46228, barva šedá","500ks",4.0823749030435961,{"$f":"F190*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735000196"]
["TECHNIK","DI  0,75- 8 šedá 100",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 8mm, dle DIN46228, barva šedá (100ks)","100ks",0.89069997884587548,{"$f":"F191*(1-Elteq!$F$9)","v":0.89069997884587548},"8591735030285"]
["TECHNIK","DI  0,75-10 bílá",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 10mm, dle DIN46228, barva bílá","500ks",8.3503123016800824,{"$f":"F192*(1-Elteq!$F$9)","v":8.3503123016800824},"8591735000202"]
["TECHNIK","DI  0,75-10 bílá 100",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 10mm, dle DIN46228, barva bílá (100ks)","100ks",1.781399957691751,{"$f":"F193*(1-Elteq!$F$9)","v":1.781399957691751},"8591735030292"]
["TECHNIK","DI  0,75-10 modrá",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 10mm, dle DIN46228, barva modrá","500ks",8.3503123016800824,{"$f":"F194*(1-Elteq!$F$9)","v":8.3503123016800824},"8591735000219"]
["TECHNIK","DI  0,75-10 modrá100",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 10mm, dle DIN46228, barva modrá (100ks)","100ks",1.781399957691751,{"$f":"F195*(1-Elteq!$F$9)","v":1.781399957691751},"8591735046125"]
["TECHNIK","DI  0,75-10 šedá",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 10mm, dle DIN46228, barva šedá","500ks",8.3503123016800824,{"$f":"F196*(1-Elteq!$F$9)","v":8.3503123016800824},"8591735000226"]
["TECHNIK","DI  0,75-12 bílá",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 12mm, dle DIN46228, barva bílá","500ks",9.649249770830318,{"$f":"F197*(1-Elteq!$F$9)","v":9.649249770830318},"8591735000233"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"DI  0,75-12 bílá 100",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 12mm, dle DIN46228, barva bílá (100ks)","100ks",2.0782999506403761,{"$f":"F198*(1-Elteq!$F$9)","v":2.0782999506403761},"8591735018405"]
["TECHNIK","DI  0,75-12 modrá",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 12mm, dle DIN46228, barva modrá","500ks",9.649249770830318,{"$f":"F199*(1-Elteq!$F$9)","v":9.649249770830318},"8591735000240"]
["TECHNIK","DI  0,75-12 šedá",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 12mm, dle DIN46228, barva šedá","500ks",9.649249770830318,{"$f":"F200*(1-Elteq!$F$9)","v":9.649249770830318},"8591735000257"]
["TECHNIK","DI  0,75-18 bílá",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 18mm, dle DIN46228, barva bílá","500ks",12.247124709130787,{"$f":"F201*(1-Elteq!$F$9)","v":12.247124709130787},"8591735030704"]
["TECHNIK","DI  1,0- 6 rudá",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 6mm, dle DIN46228, barva rudá","500ks",6.6802498413440663,{"$f":"F202*(1-Elteq!$F$9)","v":6.6802498413440663},"8591735000264"]
["TECHNIK","DI  1,0- 6 rudá 100",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 6mm, dle DIN46228, barva rudá (100ks)","100ks",1.4844999647431258,{"$f":"F203*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735017408"]
["TECHNIK","DI  1,0- 6 žlutá",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 6mm, dle DIN46228, barva žlutá","500ks",6.6802498413440663,{"$f":"F204*(1-Elteq!$F$9)","v":6.6802498413440663},"8591735000271"]
["TECHNIK","DI  1,0- 6 žlutá 100",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 6mm, dle DIN46228, barva žlutá (100ks)","100ks",1.4844999647431258,{"$f":"F205*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735030308"]
["TECHNIK","DI  1,0- 8 rudá",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 8mm, dle DIN46228, barva rudá","500ks",4.0823749030435961,{"$f":"F206*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735000288"]
["TECHNIK","DI  1,0- 8 rudá 100",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 8mm, dle DIN46228, barva rudá (100ks)","100ks",0.89069997884587548,{"$f":"F207*(1-Elteq!$F$9)","v":0.89069997884587548},"8591735017415"]
["TECHNIK","DI  1,0- 8 žlutá",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 8mm, dle DIN46228, barva žlutá","500ks",4.0823749030435961,{"$f":"F208*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735000295"]
["TECHNIK","DI  1,0- 8 žlutá 100",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 8mm, dle DIN46228, barva žlutá (100ks)","100ks",0.89069997884587548,{"$f":"F209*(1-Elteq!$F$9)","v":0.89069997884587548},"8591735017439"]
["TECHNIK","DI  1,0-10 rudá",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 10mm, dle DIN46228, barva rudá","500ks",7.274049827241317,{"$f":"F210*(1-Elteq!$F$9)","v":7.274049827241317},"8591735000301"]
["TECHNIK","DI  1,0-10 rudá 100",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 10mm, dle DIN46228, barva rudá (100ks)","100ks",1.5958374620988602,{"$f":"F211*(1-Elteq!$F$9)","v":1.5958374620988602},"8591735010003"]
["TECHNIK","DI  1,0-10 žlutá",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 10mm, dle DIN46228, barva žlutá","500ks",7.274049827241317,{"$f":"F212*(1-Elteq!$F$9)","v":7.274049827241317},"8591735000318"]
["TECHNIK","DI  1,0-10 žlutá 100",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 10mm, dle DIN46228, barva žlutá (100ks)","100ks",1.5958374620988602,{"$f":"F213*(1-Elteq!$F$9)","v":1.5958374620988602},"8591735030179"]
["TECHNIK","DI  1,0-12 rudá",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 12mm, dle DIN46228, barva rudá","500ks",9.649249770830318,{"$f":"F214*(1-Elteq!$F$9)","v":9.649249770830318},"8591735000325"]
["TECHNIK","DI  1,0-12 rudá 100",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 12mm, dle DIN46228, barva rudá (100ks)","100ks",2.0782999506403761,{"$f":"F215*(1-Elteq!$F$9)","v":2.0782999506403761},"8591735018412"]
["TECHNIK","DI  1,0-12 žlutá",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 12mm, dle DIN46228, barva žlutá","500ks",9.649249770830318,{"$f":"F216*(1-Elteq!$F$9)","v":9.649249770830318},"8591735000332"]
["TECHNIK","DI  1,0-12 žlutá 100",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 12mm, dle DIN46228, barva žlutá (100ks)","100ks",2.0782999506403761,{"$f":"F217*(1-Elteq!$F$9)","v":2.0782999506403761},"8591735033293"]
["TECHNIK","DI  1,0-18 žlutá",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 18mm, dle DIN46228, barva žlutá","500ks",12.247124709130787,{"$f":"F218*(1-Elteq!$F$9)","v":12.247124709130787},"8591735030711"]
["TECHNIK","DI  1,5- 6 černá",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 6mm, dle DIN46228, barva černá","500ks",6.6802498413440663,{"$f":"F219*(1-Elteq!$F$9)","v":6.6802498413440663},"8591735000349"]
["TECHNIK","DI  1,5- 6 rudá",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 6mm, dle DIN46228, barva rudá","500ks",6.6802498413440663,{"$f":"F220*(1-Elteq!$F$9)","v":6.6802498413440663},"8591735000356"]
["TECHNIK","DI  1,5- 6 rudá 100",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 6mm, dle DIN46228, barva rudá (100ks)","100ks",1.4844999647431258,{"$f":"F221*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735030315"]
["TECHNIK","DI  1,5- 8 černá",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 8mm, dle DIN46228, barva černá","500ks",4.0823749030435961,{"$f":"F222*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735000363"]
["TECHNIK","DI  1,5- 8 černá 100",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 8mm, dle DIN46228, barva černá (100ks)","100ks",0.89069997884587548,{"$f":"F223*(1-Elteq!$F$9)","v":0.89069997884587548},"8591735017422"]
["TECHNIK","DI  1,5- 8 rudá",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 8mm, dle DIN46228, barva rudá","500ks",4.0823749030435961,{"$f":"F224*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735000370"]
["TECHNIK","DI  1,5- 8 rudá 100",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 8mm, dle DIN46228, barva rudá (100ks)","100ks",0.89069997884587548,{"$f":"F225*(1-Elteq!$F$9)","v":0.89069997884587548},"8591735017446"]
["TECHNIK","DI  1,5-10 černá",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 10mm, dle DIN46228, barva černá","500ks",7.274049827241317,{"$f":"F226*(1-Elteq!$F$9)","v":7.274049827241317},"8591735000387"]
["TECHNIK","DI  1,5-10 černá 100",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 10mm, dle DIN46228, barva černá (100ks)","100ks",1.5958374620988602,{"$f":"F227*(1-Elteq!$F$9)","v":1.5958374620988602},"8591735018252"]
["TECHNIK","DI  1,5-10 rudá",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 10mm, dle DIN46228, barva rudá","500ks",7.274049827241317,{"$f":"F228*(1-Elteq!$F$9)","v":7.274049827241317},"8591735000394"]
["TECHNIK","DI  1,5-10 rudá 100",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 10mm, dle DIN46228, barva rudá (100ks)","100ks",1.5958374620988602,{"$f":"F229*(1-Elteq!$F$9)","v":1.5958374620988602},"8591735030186"]
["TECHNIK","DI  1,5-12 černá",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 12mm, dle DIN46228, barva černá","500ks",10.020374762016099,{"$f":"F230*(1-Elteq!$F$9)","v":10.020374762016099},"8591735000400"]
["TECHNIK","DI  1,5-12 černá 100",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 12mm, dle DIN46228, barva černá (100ks)","100ks",2.1896374479961107,{"$f":"F231*(1-Elteq!$F$9)","v":2.1896374479961107},"8591735047184"]
["TECHNIK","DI  1,5-12 rudá",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 12mm, dle DIN46228, barva rudá","500ks",10.020374762016099,{"$f":"F232*(1-Elteq!$F$9)","v":10.020374762016099},"8591735000417"]
["TECHNIK","DI  1,5-12 rudá 100",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 12mm, dle DIN46228, barva rudá (100ks)","100ks",2.1896374479961107,{"$f":"F233*(1-Elteq!$F$9)","v":2.1896374479961107},"8591735018429"]
["TECHNIK","DI  1,5-18 černá",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 18mm, dle DIN46228, barva černá","500ks",11.875999717945007,{"$f":"F234*(1-Elteq!$F$9)","v":11.875999717945007},"8591735010584"]
["TECHNIK","DI  1,5-18 černá 100",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 18mm, dle DIN46228, barva černá (100ks)","100ks",2.5978749383004702,{"$f":"F235*(1-Elteq!$F$9)","v":2.5978749383004702},"8591735050771"]
["TECHNIK","DI  1,5-18 rudá",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 18mm, dle DIN46228, barva rudá","500ks",11.875999717945007,{"$f":"F236*(1-Elteq!$F$9)","v":11.875999717945007},"8591735010577"]
["TECHNIK","DI  1,5-18 rudá 100",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 18mm, dle DIN46228, barva rudá (100ks)","100ks",2.5978749383004702,{"$f":"F237*(1-Elteq!$F$9)","v":2.5978749383004702},"8591735030322"]
["TECHNIK","DI  2,5- 6 modrá",null,"Dutinka izolovaná, průřez 2,5mm2 / délka 6mm, dle DIN46228, barva modrá","500ks",8.5358747972729727,{"$f":"F238*(1-Elteq!$F$9)","v":8.5358747972729727},"8591735050863"]
["TECHNIK","DI  2,5- 8 modrá",null,"Dutinka izolovaná, průřez 2,5mm2 / délka 8mm, dle DIN46228, barva modrá","500ks",4.6390623898222678,{"$f":"F239*(1-Elteq!$F$9)","v":4.6390623898222678},"8591735000424"]
["TECHNIK","DI  2,5- 8 modrá 100",null,"Dutinka izolovaná, průřez 2,5mm2 / délka 8mm, dle DIN46228, barva modrá (100ks)","100ks",0.96492497708303182,{"$f":"F240*(1-Elteq!$F$9)","v":0.96492497708303182},"8591735030339"]
["TECHNIK","DI  2,5- 8 šedá",null,"Dutinka izolovaná, průřez 2,5mm2 / délka 8mm, dle DIN46228, barva šedá","500ks",4.6390623898222678,{"$f":"F241*(1-Elteq!$F$9)","v":4.6390623898222678},"8591735000431"]
["TECHNIK","DI  2,5- 8 šedá 100",null,"Dutinka izolovaná, průřez 2,5mm2 / délka 8mm, dle DIN46228, barva šedá (100ks)","100ks",0.96492497708303182,{"$f":"F242*(1-Elteq!$F$9)","v":0.96492497708303182},"8591735017699"]
["TECHNIK","DI  2,5-10 modrá",null,"Dutinka izolovaná, průřez 2,5mm2 / délka 10mm, dle DIN46228, barva modrá","500ks",8.9069997884587551,{"$f":"F243*(1-Elteq!$F$9)","v":8.9069997884587551},"8591735011567"]
["TECHNIK","DI  2,5-10 modrá 100",null,"Dutinka izolovaná, průřez 2,5mm2 / délka 10mm, dle DIN46228, barva modrá (100ks)","100ks",1.781399957691751,{"$f":"F244*(1-Elteq!$F$9)","v":1.781399957691751},"8591735030346"]
["TECHNIK","DI  2,5-10 šedá",null,"Dutinka izolovaná, průřez 2,5mm2 / délka 10mm, dle DIN46228, barva šedá","500ks",8.9069997884587551,{"$f":"F245*(1-Elteq!$F$9)","v":8.9069997884587551},"8591735014551"]
["TECHNIK","DI  2,5-12 modrá",null,"Dutinka izolovaná, průřez 2,5mm2 / délka 12mm, dle DIN46228, barva modrá","500ks",10.020374762016099,{"$f":"F246*(1-Elteq!$F$9)","v":10.020374762016099},"8591735000448"]
["TECHNIK","DI  2,5-12 modrá 100",null,"Dutinka izolovaná, průřez 2,5mm2 / délka 12mm, dle DIN46228, barva modrá (100ks)","100ks",2.1154124497589541,{"$f":"F247*(1-Elteq!$F$9)","v":2.1154124497589541},"8591735017507"]
["TECHNIK","DI  2,5-12 šedá",null,"Dutinka izolovaná, průřez 2,5mm2 / délka 12mm, dle DIN46228, barva šedá","500ks",10.020374762016099,{"$f":"F248*(1-Elteq!$F$9)","v":10.020374762016099},"8591735000455"]
["TECHNIK","DI  2,5-18 modrá",null,"Dutinka izolovaná, průřez 2,5mm2 / délka 18mm, dle DIN46228, barva modrá","500ks",12.98937469150235,{"$f":"F249*(1-Elteq!$F$9)","v":12.98937469150235},"8591735000462"]
["TECHNIK","DI  2,5-18 modrá 100",null,"Dutinka izolovaná, průřez 2,5mm2 / délka 18mm, dle DIN46228, barva modrá (100ks)","100ks",2.7463249347747829,{"$f":"F250*(1-Elteq!$F$9)","v":2.7463249347747829},"8591735030353"]
["TECHNIK","DI  2,5-18 šedá",null,"Dutinka izolovaná, průřez 2,5mm2 / délka 18mm, dle DIN46228, barva šedá","500ks",12.98937469150235,{"$f":"F251*(1-Elteq!$F$9)","v":12.98937469150235},"8591735010454"]
["TECHNIK","DI  2,5-25 modrá",null,"Dutinka izolovaná, průřez 2,5mm2 / délka 25mm, dle DIN46228, barva modrá","500ks",15.030562143024149,{"$f":"F252*(1-Elteq!$F$9)","v":15.030562143024149},"8591735030728"]
["TECHNIK","DI  4-10 oranž 100",null,"Dutinka izolovaná, průřez 4,0mm2 / délka 10mm, dle DIN46228, barva oranžová (100ks)","100ks",1.781399957691751,{"$f":"F253*(1-Elteq!$F$9)","v":1.781399957691751},"8591735030797"]
["TECHNIK","DI  4-10 oranžová",null,"Dutinka izolovaná, průřez 4,0mm2 / délka 10mm, dle DIN46228, barva oranžová","500ks",8.5729872963915525,{"$f":"F254*(1-Elteq!$F$9)","v":8.5729872963915525},"8591735000479"]
["TECHNIK","DI  4-10 šedá",null,"Dutinka izolovaná, průřez 4,0mm2 / délka 10mm, dle DIN46228, barva šedá","500ks",8.5729872963915525,{"$f":"F255*(1-Elteq!$F$9)","v":8.5729872963915525},"8591735000486"]
["TECHNIK","DI  4-10 šedá 100",null,"Dutinka izolovaná, průřez 4,0mm2 / délka 10mm, dle DIN46228, barva šedá (100ks)","100ks",1.781399957691751,{"$f":"F256*(1-Elteq!$F$9)","v":1.781399957691751},"8591735030360"]
["TECHNIK","DI  4-12 oranž 100",null,"Dutinka izolovaná, průřez 4,0mm2 / délka 12mm, dle DIN46228, barva oranžová (100ks)","100ks",2.4865374409447356,{"$f":"F257*(1-Elteq!$F$9)","v":2.4865374409447356},"8591735017514"]
["TECHNIK","DI  4-12 oranžová",null,"Dutinka izolovaná, průřez 4,0mm2 / délka 12mm, dle DIN46228, barva oranžová","500ks",11.690437222352116,{"$f":"F258*(1-Elteq!$F$9)","v":11.690437222352116},"8591735000493"]
["TECHNIK","DI  4-12 šedá",null,"Dutinka izolovaná, průřez 4,0mm2 / délka 12mm, dle DIN46228, barva šedá","500ks",11.690437222352116,{"$f":"F259*(1-Elteq!$F$9)","v":11.690437222352116},"8591735000509"]
["TECHNIK","DI  4-12 šedá 100",null,"Dutinka izolovaná, průřez 4,0mm2 / délka 12mm, dle DIN46228, barva šedá (100ks)","100ks",2.4865374409447356,{"$f":"F260*(1-Elteq!$F$9)","v":2.4865374409447356},"8591735018337"]
["TECHNIK","DI  4-18 oranžová",null,"Dutinka izolovaná, průřez 4,0mm2 / délka 18mm, dle DIN46228, barva oranžová","100ks",3.5442436658242129,{"$f":"F261*(1-Elteq!$F$9)","v":3.5442436658242129},"8591735000516"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"DI  4-18 šedá",null,"Dutinka izolovaná, průřez 4,0mm2 / délka 18mm, dle DIN46228, barva šedá","100ks",3.5442436658242129,{"$f":"F262*(1-Elteq!$F$9)","v":3.5442436658242129},"8591735000523"]
["TECHNIK","DI  6-12 černá",null,"Dutinka izolovaná, průřez 6,0mm2 / délka 12mm, dle DIN46228, barva černá","100ks",2.4494249418261576,{"$f":"F263*(1-Elteq!$F$9)","v":2.4494249418261576},"8591735000530"]
["TECHNIK","DI  6-12 zelená",null,"Dutinka izolovaná, průřez 6,0mm2 / délka 12mm, dle DIN46228, barva zelená","100ks",2.4494249418261576,{"$f":"F264*(1-Elteq!$F$9)","v":2.4494249418261576},"8591735000547"]
["TECHNIK","DI  6-12 žlutá",null,"Dutinka izolovaná, průřez 6,0mm2 / délka 12mm, dle DIN46228, barva žlutá","100ks",2.4494249418261576,{"$f":"F265*(1-Elteq!$F$9)","v":2.4494249418261576},"8591735000554"]
["TECHNIK","DI  6-18 černá",null,"Dutinka izolovaná, průřez 6,0mm2 / délka 18mm, dle DIN46228, barva černá","100ks",3.9339249065692834,{"$f":"F266*(1-Elteq!$F$9)","v":3.9339249065692834},"8591735000561"]
["TECHNIK","DI  6-18 zelená",null,"Dutinka izolovaná, průřez 6,0mm2 / délka 18mm, dle DIN46228, barva zelená","100ks",3.9339249065692834,{"$f":"F267*(1-Elteq!$F$9)","v":3.9339249065692834},"8591735000578"]
["TECHNIK","DI  6-18 žlutá",null,"Dutinka izolovaná, průřez 6,0mm2 / délka 18mm, dle DIN46228, barva žlutá","100ks",3.9339249065692834,{"$f":"F268*(1-Elteq!$F$9)","v":3.9339249065692834},"8591735022440"]
["TECHNIK","DI 10-12 hnědá",null,"Dutinka izolovaná, průřez 10mm2 / délka 12mm, dle DIN46228, barva hnědá","100ks",3.3772374197906112,{"$f":"F269*(1-Elteq!$F$9)","v":3.3772374197906112},"8591735000592"]
["TECHNIK","DI 10-12 rudá",null,"Dutinka izolovaná, průřez 10mm2 / délka 12mm, dle DIN46228, barva rudá","100ks",3.3772374197906112,{"$f":"F270*(1-Elteq!$F$9)","v":3.3772374197906112},"8591735000608"]
["TECHNIK","DI 10-12 sl. kost",null,"Dutinka izolovaná, průřez 10mm2 / délka 12mm, dle DIN46228, barva sl. kost","100ks",3.3772374197906112,{"$f":"F271*(1-Elteq!$F$9)","v":3.3772374197906112},"8591735000585"]
["TECHNIK","DI 10-18 hnědá",null,"Dutinka izolovaná, průřez 10mm2 / délka 18mm, dle DIN46228, barva hnědá","100ks",5.0101873810080493,{"$f":"F272*(1-Elteq!$F$9)","v":5.0101873810080493},"8591735000622"]
["TECHNIK","DI 10-18 rudá",null,"Dutinka izolovaná, průřez 10mm2 / délka 18mm, dle DIN46228, barva rudá","100ks",5.0101873810080493,{"$f":"F273*(1-Elteq!$F$9)","v":5.0101873810080493},"8591735015626"]
["TECHNIK","DI 10-18 sl. kost",null,"Dutinka izolovaná, průřez 10mm2 / délka 18mm, dle DIN46228, barva sl. kost","100ks",5.0101873810080493,{"$f":"F274*(1-Elteq!$F$9)","v":5.0101873810080493},"8591735000615"]
["TECHNIK","DI 16-12 bílá",null,"Dutinka izolovaná, průřez 16mm2 / délka 12mm, dle DIN46228, barva bílá","100ks",5.1957498766009405,{"$f":"F275*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735000639"]
["TECHNIK","DI 16-12 modrá",null,"Dutinka izolovaná, průřez 16mm2 / délka 12mm, dle DIN46228, barva modrá","100ks",5.1957498766009405,{"$f":"F276*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735000646"]
["TECHNIK","DI 16-12 zelená",null,"Dutinka izolovaná, průřez 16mm2 / délka 12mm, dle DIN46228, barva zelená","100ks",5.1957498766009405,{"$f":"F277*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735000653"]
["TECHNIK","DI 16-18 bílá",null,"Dutinka izolovaná, průřez 16mm2 / délka 18mm, dle DIN46228, barva bílá","100ks",6.6431373422254882,{"$f":"F278*(1-Elteq!$F$9)","v":6.6431373422254882},"8591735000660"]
["TECHNIK","DI 16-18 modrá",null,"Dutinka izolovaná, průřez 16mm2 / délka 18mm, dle DIN46228, barva modrá","100ks",6.6431373422254882,{"$f":"F279*(1-Elteq!$F$9)","v":6.6431373422254882},"8591735000677"]
["TECHNIK","DI 16-18 zelená",null,"Dutinka izolovaná, průřez 16mm2 / délka 18mm, dle DIN46228, barva zelená","100ks",6.6431373422254882,{"$f":"F280*(1-Elteq!$F$9)","v":6.6431373422254882},"8591735000684"]
["TECHNIK","DI 25-16 černá",null,"Dutinka izolovaná, průřez 25mm2 / délka 16mm, dle DIN46228, barva černá","50ks",5.2885311243973856,{"$f":"F281*(1-Elteq!$F$9)","v":5.2885311243973856},"8591735000691"]
["TECHNIK","DI 25-16 hnědá",null,"Dutinka izolovaná, průřez 25mm2 / délka 16mm, dle DIN46228, barva hnědá","50ks",5.2885311243973856,{"$f":"F282*(1-Elteq!$F$9)","v":5.2885311243973856},"8591735000707"]
["TECHNIK","DI 25-16 žlutá",null,"Dutinka izolovaná, průřez 25mm2 / délka 16mm, dle DIN46228, barva žlutá","50ks",5.2885311243973856,{"$f":"F283*(1-Elteq!$F$9)","v":5.2885311243973856},"8591735009465"]
["TECHNIK","DI 25-18 hnědá",null,"Dutinka izolovaná, průřez 25mm2 / délka 18mm, dle DIN46228, barva hnědá","50ks",6.1235623545653937,{"$f":"F284*(1-Elteq!$F$9)","v":6.1235623545653937},"8591735013240"]
["TECHNIK","DI 25-22 černá",null,"Dutinka izolovaná, průřez 25mm2 / délka 22mm, dle DIN46228, barva černá","50ks",8.1647498060871921,{"$f":"F285*(1-Elteq!$F$9)","v":8.1647498060871921},"8591735000714"]
["TECHNIK","DI 25-22 hnědá",null,"Dutinka izolovaná, průřez 25mm2 / délka 22mm, dle DIN46228, barva hnědá","50ks",8.1647498060871921,{"$f":"F286*(1-Elteq!$F$9)","v":8.1647498060871921},"8591735000721"]
["TECHNIK","DI 25-22 žlutá",null,"Dutinka izolovaná, průřez 25mm2 / délka 22mm, dle DIN46228, barva žlutá","50ks",8.1647498060871921,{"$f":"F287*(1-Elteq!$F$9)","v":8.1647498060871921},"8591735019020"]
["TECHNIK","DI 35-16 béžová",null,"Dutinka izolovaná, průřez 35mm2 / délka 16mm, dle DIN46228, barva béžová","50ks",6.3647935988361519,{"$f":"F288*(1-Elteq!$F$9)","v":6.3647935988361519},"8591735000738"]
["TECHNIK","DI 35-16 rudá",null,"Dutinka izolovaná, průřez 35mm2 / délka 16mm, dle DIN46228, barva rudá","50ks",6.3647935988361519,{"$f":"F289*(1-Elteq!$F$9)","v":6.3647935988361519},"8591735000745"]
["TECHNIK","DI 35-18 béžová",null,"Dutinka izolovaná, průřez 35mm2 / délka 18mm, dle DIN46228, barva béžová","50ks",7.19982482900416,{"$f":"F290*(1-Elteq!$F$9)","v":7.19982482900416},"8591735013257"]
["TECHNIK","DI 35-25 béžová",null,"Dutinka izolovaná, průřez 35mm2 / délka 25mm, dle DIN46228, barva béžová","50ks",11.02241223821771,{"$f":"F291*(1-Elteq!$F$9)","v":11.02241223821771},"8591735000752"]
["TECHNIK","DI 35-25 rudá",null,"Dutinka izolovaná, průřez 35mm2 / délka 25mm, dle DIN46228, barva rudá","50ks",11.02241223821771,{"$f":"F292*(1-Elteq!$F$9)","v":11.02241223821771},"8591735000769"]
["TECHNIK","DI 50-20 modrá",null,"Dutinka izolovaná, průřez 50mm2 / délka 20mm, dle DIN46228, barva modrá","50ks",9.3523497778816935,{"$f":"F293*(1-Elteq!$F$9)","v":9.3523497778816935},"8591735000776"]
["TECHNIK","DI 50-20 zelená",null,"Dutinka izolovaná, průřez 50mm2 / délka 20mm, dle DIN46228, barva zelená","50ks",9.3523497778816935,{"$f":"F294*(1-Elteq!$F$9)","v":9.3523497778816935},"8591735000783"]
["TECHNIK","DI 50-25 modrá",null,"Dutinka izolovaná, průřez 50mm2 / délka 25mm, dle DIN46228, barva modrá","50ks",14.844999647431258,{"$f":"F295*(1-Elteq!$F$9)","v":14.844999647431258},"8591735022457"]
["TECHNIK","DI 50-25 zelená",null,"Dutinka izolovaná, průřez 50mm2 / délka 25mm, dle DIN46228, barva zelená","50ks",14.844999647431258,{"$f":"F296*(1-Elteq!$F$9)","v":14.844999647431258},"8591735000790"]
["TECHNIK","DI 50-30 zelená",null,"Dutinka izolovaná, průřez 50mm2 / délka 30mm, dle DIN46228, barva zelená","50ks",15.513024631565665,{"$f":"F297*(1-Elteq!$F$9)","v":15.513024631565665},"8591735030735"]
["TECHNIK","DI 70-20 žlutá",null,"Dutinka izolovaná, průřez 70mm2 / délka 20mm, dle DIN46228, barva žlutá","25ks",8.2575310538836373,{"$f":"F298*(1-Elteq!$F$9)","v":8.2575310538836373},"8591735000806"]
["TECHNIK","DI 70-25 žlutá",null,"Dutinka izolovaná, průřez 70mm2 / délka 25mm, dle DIN46228, barva žlutá","25ks",11.02241223821771,{"$f":"F299*(1-Elteq!$F$9)","v":11.02241223821771},"8591735030742"]
["TECHNIK","DI 95-25 rudá",null,"Dutinka izolovaná, průřez 95mm2 / délka 25mm, dle DIN46228, barva rudá","25ks",13.174937187095242,{"$f":"F300*(1-Elteq!$F$9)","v":13.174937187095242},"8591735000813"]
["TECHNIK","DI 95-30 rudá",null,"Dutinka izolovaná, průřez 95mm2 / délka 30mm, dle DIN46228, barva rudá","25ks",15.513024631565665,{"$f":"F301*(1-Elteq!$F$9)","v":15.513024631565665},"8591735030759"]
["TECHNIK","DI120-27 modrá",null,"Dutinka izolovaná, průřez 120mm2 / délka 27mm, dle DIN46228, barva modrá","25ks",14.473874656245476,{"$f":"F302*(1-Elteq!$F$9)","v":14.473874656245476},"8591735000820"]
["TECHNIK","DI120-34 modrá",null,"Dutinka izolovaná, průřez 120mm2 / délka 34mm, dle DIN46228, barva modrá","25ks",20.040749524032197,{"$f":"F303*(1-Elteq!$F$9)","v":20.040749524032197},"8591735030766"]
["TECHNIK","DI150-32 žlutá",null,"Dutinka izolovaná, průřez 150mm2 / délka 32mm, dle DIN46228, barva žlutá","25ks",15.958374620988602,{"$f":"F304*(1-Elteq!$F$9)","v":15.958374620988602},"8591735000837"]
["TECHNIK","DIF  2,5- 8 modrá",null,"Dutinka izolovaná s rozšířeným límcem 7,3mm / průřez 2,5mm2 / délka 8mm, barva modrá","100ks",4.824624885415159,{"$f":"F305*(1-Elteq!$F$9)","v":4.824624885415159},"8591735035792"]
["TECHNIK","DIF  2,5-12 modrá",null,"Dutinka izolovaná s rozšířeným límcem 7,3mm / průřez 2,5mm2 / délka 12mm, barva modrá","100ks",5.8266623616167692,{"$f":"F306*(1-Elteq!$F$9)","v":5.8266623616167692},"8591735030773"]
["TECHNIK","DIF  4-10 šedá",null,"Dutinka izolovaná s rozšířeným límcem 7,3mm / průřez 4,0mm2 / délka 10mm, barva šedá","100ks",6.8658123369369566,{"$f":"F307*(1-Elteq!$F$9)","v":6.8658123369369566},"8591735030780"]
["TECHNIK","DIF 16-12 modrá",null,"Dutinka izolovaná s rozšířeným límcem 11,9mm / průřez 4,0mm2 / délka 10mm, barva modrá","100ks",11.987337215300741,{"$f":"F308*(1-Elteq!$F$9)","v":11.987337215300741},"8591735030872"]
["TECHNIK","DIZ  1,5- 8 černá",null,"Dutinka izolovaná s rozšířeným límcem 7,5mm / průřez 1,5mm2 / délka 8mm, barva černá","100ks",3.0061124286048297,{"$f":"F309*(1-Elteq!$F$9)","v":3.0061124286048297},"8591735051105"]
["TECHNIK","DIZ  1,5-10 černá",null,"Dutinka izolovaná s rozšířeným límcem 7,5mm / průřez 1,5mm2 / délka 10mm, barva černá","100ks",3.3401249206720331,{"$f":"F310*(1-Elteq!$F$9)","v":3.3401249206720331},"8591735051112"]
["TECHNIK","DIZ  2,5- 8 modrá",null,"Dutinka izolovaná s rozšířeným límcem 8,0mm / průřez 2,5mm2 / délka 8mm, barva modrá","100ks",3.3401249206720331,{"$f":"F311*(1-Elteq!$F$9)","v":3.3401249206720331},"8591735030902"]
["TECHNIK","DIZ  2,5-12 modrá",null,"Dutinka izolovaná s rozšířeným límcem 8,0mm / průřez 2,5mm2 / délka 12mm, barva modrá","100ks",3.8968124074507053,{"$f":"F312*(1-Elteq!$F$9)","v":3.8968124074507053},"8591735030919"]
["TECHNIK","DIZ  4-10 šedá",null,"Dutinka izolovaná s rozšířeným límcem 9,5mm / průřez 4,0mm2 / délka 10mm, barva šedá","100ks",3.8968124074507053,{"$f":"F313*(1-Elteq!$F$9)","v":3.8968124074507053},"8591735030926"]
["TECHNIK","DIZ  6-12 černá",null,"Dutinka izolovaná s rozšířeným límcem 10,0mm / průřez 6,0mm2 / délka 12mm, barva černá","100ks",5.3813123721938307,{"$f":"F314*(1-Elteq!$F$9)","v":5.3813123721938307},"8591735030933"]
["TECHNIK","DIZ 10-12 rudá",null,"Dutinka izolovaná s rozšířeným límcem 11,5mm / průřez 10mm2 / délka 12mm, barva rudá","100ks",7.5338373210713634,{"$f":"F315*(1-Elteq!$F$9)","v":7.5338373210713634},"8591735030940"]
["TECHNIK","DIZ 16-12 modrá",null,"Dutinka izolovaná s rozšířeným límcem 13,5mm / průřez 16mm2 / délka 12mm, barva modrá","100ks",8.3874248007986605,{"$f":"F316*(1-Elteq!$F$9)","v":8.3874248007986605},"8591735030957"]
["TECHNIK","DP 0,5- 8 bílá",null,"Dutinka izolovaná, průřez 0,50mm2 / délka 8mm, barva bílá (10x50ks)","500ks",6.3091248501582848,{"$f":"F317*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735001162"]
["TECHNIK","DP 0,5- 8 oranžová",null,"Dutinka izolovaná, průřez 0,50mm2 / délka 8mm, barva oranžová (10x50ks)","500ks",6.3091248501582848,{"$f":"F318*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735001179"]
["TECHNIK","DP 0,75- 8 bílá",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 8mm, barva bílá (10x50ks)","500ks",6.3091248501582848,{"$f":"F319*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735001186"]
["TECHNIK","DP 0,75- 8 šedá",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 8mm, barva šedá (10x50ks)","500ks",6.3091248501582848,{"$f":"F320*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735001193"]
["TECHNIK","DP 0,75-8 modrá",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 8mm, barva modrá (10x50ks)","500ks",6.3091248501582848,{"$f":"F321*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735010829"]
["TECHNIK","DP 1,0- 8 rudá",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 8mm, barva rudá (10x50ks)","500ks",6.3091248501582848,{"$f":"F322*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735001209"]
["TECHNIK","DP 1,0- 8 žlutá",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 8mm, barva žlutá (10x50ks)","500ks",6.3091248501582848,{"$f":"F323*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735001216"]
["TECHNIK","DP 1,5- 8 černá",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 8mm, barva černá (10x50ks)","500ks",6.3091248501582848,{"$f":"F324*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735001223"]
["TECHNIK","DP 1,5- 8 rudá",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 8mm, barva rudá (10x50ks)","500ks",6.3091248501582848,{"$f":"F325*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735001230"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"DP 2,5- 8 modrá",null,"Dutinka izolovaná, průřez 2,5mm2 / délka 8mm, barva modrá (10x50ks)","500ks",7.979187310494301,{"$f":"F326*(1-Elteq!$F$9)","v":7.979187310494301},"8591735001247"]
["TECHNIK","DP 2,5- 8 šedá",null,"Dutinka izolovaná, průřez 2,5mm2 / délka 8mm, barva šedá (10x50ks)","500ks",7.979187310494301,{"$f":"F327*(1-Elteq!$F$9)","v":7.979187310494301},"8591735001254"]
["TECHNIK","DRMC 0,25-8 modrá",null,"Dutinka izolovaná, průřez 0,25mm2 / délka 8mm, barva modrá (cívka)","1000ks",16.329499612174384,{"$f":"F328*(1-Elteq!$F$9)","v":16.329499612174384},"8591735038410"]
["TECHNIK","DRMC 0,34-8 tyrkys",null,"Dutinka izolovaná, průřez 0,34mm2 / délka 8mm, barva tyrkysová (cívka)","1000ks",16.329499612174384,{"$f":"F329*(1-Elteq!$F$9)","v":16.329499612174384},"8591735038427"]
["TECHNIK","DRMC 0,5-8 bílá",null,"Dutinka izolovaná, průřez 0,50mm2 / délka 8mm, barva bílá (cívka)","1000ks",14.473874656245476,{"$f":"F330*(1-Elteq!$F$9)","v":14.473874656245476},"8591735040635"]
["TECHNIK","DRMC 0,5-8 oranžová",null,"Dutinka izolovaná, průřez 0,50mm2 / délka 8mm, barva oranžová (cívka)","1000ks",14.473874656245476,{"$f":"F331*(1-Elteq!$F$9)","v":14.473874656245476},"8591735030803"]
["TECHNIK","DRMC 0,75-8 bílá",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 8mm, barva bílá (cívka)","1000ks",14.473874656245476,{"$f":"F332*(1-Elteq!$F$9)","v":14.473874656245476},"8591735030810"]
["TECHNIK","DRMC 0,75-8 šedá",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 8mm, barva šedá (cívka)","1000ks",14.473874656245476,{"$f":"F333*(1-Elteq!$F$9)","v":14.473874656245476},"8591735037123"]
["TECHNIK","DRMC 1,0-8 rudá",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 8mm, barva rudá (cívka)","1000ks",14.473874656245476,{"$f":"F334*(1-Elteq!$F$9)","v":14.473874656245476},"8591735030827"]
["TECHNIK","DRMC 1,0-8 žlutá",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 8mm, barva žlutá (cívka)","1000ks",14.473874656245476,{"$f":"F335*(1-Elteq!$F$9)","v":14.473874656245476},"8591735030834"]
["TECHNIK","DRMC 1,5-8 černá",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 8mm, barva černá (cívka)","1000ks",14.473874656245476,{"$f":"F336*(1-Elteq!$F$9)","v":14.473874656245476},"8591735040642"]
["TECHNIK","DRMC 1,5-8 rudá",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 8mm, barva rudá (cívka)","1000ks",14.473874656245476,{"$f":"F337*(1-Elteq!$F$9)","v":14.473874656245476},"8591735030841"]
["TECHNIK","DRMC 2,5-8 modrá",null,"Dutinka izolovaná, průřez 2,5mm2 / délka 8mm, barva modrá (cívka)","500ks",8.9069997884587551,{"$f":"F338*(1-Elteq!$F$9)","v":8.9069997884587551},"8591735030858"]
["TECHNIK","DRS 0,34-8 tyrkysová",null,"Dutinka izolovaná, průřez 0,34mm2 / délka 8mm, barva tyrkysová (cívka 5000ks)","5000ks",79.791873104943008,{"$f":"F339*(1-Elteq!$F$9)","v":79.791873104943008},"8591735036577"]
["TECHNIK","DRS 0,5-8 bílá",null,"Dutinka izolovaná, průřez 0,50mm2 / délka 8mm, barva bílá (cívka 10000ks)","10000ks",115.79099724996381,{"$f":"F340*(1-Elteq!$F$9)","v":115.79099724996381},"8591735048648"]
["TECHNIK","DRS 0,5-8 oranžová",null,"Dutinka izolovaná, průřez 0,50mm2 / délka 8mm, barva oranžová (cívka 10000ks)","10000ks",115.79099724996381,{"$f":"F341*(1-Elteq!$F$9)","v":115.79099724996381},"8591735007393"]
["TECHNIK","DRS 0,75-8 bílá",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 8mm, barva bílá (cívka 10000ks)","10000ks",115.79099724996381,{"$f":"F342*(1-Elteq!$F$9)","v":115.79099724996381},"8591735007409"]
["TECHNIK","DRS 0,75-8 modrá",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 8mm, barva modrá (cívka 10000ks)","10000ks",115.79099724996381,{"$f":"F343*(1-Elteq!$F$9)","v":115.79099724996381},"8591735048655"]
["TECHNIK","DRS 0,75-8 šedá",null,"Dutinka izolovaná, průřez 0,75mm2 / délka 8mm, barva šedá (cívka 10000ks)","10000ks",115.79099724996381,{"$f":"F344*(1-Elteq!$F$9)","v":115.79099724996381},"8591735030865"]
["TECHNIK","DRS 1,0-8 rudá",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 8mm, barva rudá (cívka 7500ks)","7500ks",86.843247937472867,{"$f":"F345*(1-Elteq!$F$9)","v":86.843247937472867},"8591735015640"]
["TECHNIK","DRS 1,0-8 žlutá",null,"Dutinka izolovaná, průřez 1,0mm2 / délka 8mm, barva žlutá (cívka 7500ks)","7500ks",86.843247937472867,{"$f":"F346*(1-Elteq!$F$9)","v":86.843247937472867},"8591735007416"]
["TECHNIK","DRS 1,5-8 černá",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 8mm, barva černá (cívka 7500ks)","7500ks",86.843247937472867,{"$f":"F347*(1-Elteq!$F$9)","v":86.843247937472867},"8591735015657"]
["TECHNIK","DRS 1,5-8 rudá",null,"Dutinka izolovaná, průřez 1,5mm2 / délka 8mm, barva rudá (cívka 7500ks)","7500ks",86.843247937472867,{"$f":"F348*(1-Elteq!$F$9)","v":86.843247937472867},"8591735007423"]
["TECHNIK","DRS 2,5-8 modrá",null,"Dutinka izolovaná, průřez 2,5mm2 / délka 8mm, barva modrá (cívka 5000ks)","5000ks",66.245810926661989,{"$f":"F349*(1-Elteq!$F$9)","v":66.245810926661989},"8591735007430"]
["TECHNIK","DRS 2,5-8 šedá",null,"Dutinka izolovaná, průřez 2,5mm2 / délka 8mm, barva šedá (cívka 5000ks)","5000ks",66.245810926661989,{"$f":"F350*(1-Elteq!$F$9)","v":66.245810926661989},"8591735035501"]
["TECHNIK","DN  0,14- 7",null,"Dutinka neizolovaná cínovaná, průřez 0,14mm2 / délka 7mm, dle DIN46228","1000ks",10.577062248794771,{"$f":"F351*(1-Elteq!$F$9)","v":10.577062248794771},"8591735001261"]
["TECHNIK","DN  0,14- 7 / 100",null,"Dutinka neizolovaná cínovaná, průřez 0,14mm2 / délka 7mm, dle DIN46228, (100ks)","100ks",1.2618249700316571,{"$f":"F352*(1-Elteq!$F$9)","v":1.2618249700316571},"8591735017965"]
["TECHNIK","DN  0,25- 5",null,"Dutinka neizolovaná cínovaná, průřez 0,25mm2 / délka 5mm, dle DIN46228","1000ks",6.3091248501582848,{"$f":"F353*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735003791"]
["TECHNIK","DN  0,25- 5 / 100",null,"Dutinka neizolovaná cínovaná, průřez 0,25mm2 / délka 5mm, dle DIN46228, (100ks)","100ks",0.81647498060871926,{"$f":"F354*(1-Elteq!$F$9)","v":0.81647498060871926},"8591735035808"]
["TECHNIK","DN  0,25- 7",null,"Dutinka neizolovaná cínovaná, průřez 0,25mm2 / délka 7mm, dle DIN46228","1000ks",7.6080623193085195,{"$f":"F355*(1-Elteq!$F$9)","v":7.6080623193085195},"8591735001278"]
["TECHNIK","DN  0,25- 7 / 100",null,"Dutinka neizolovaná cínovaná, průřez 0,25mm2 / délka 7mm, dle DIN46228, (100ks)","100ks",0.90925622840516462,{"$f":"F356*(1-Elteq!$F$9)","v":0.90925622840516462},"8591735033286"]
["TECHNIK","DN  0,34- 5",null,"Dutinka neizolovaná cínovaná, průřez 0,34mm2 / délka 5mm, dle DIN46228","1000ks",6.3091248501582848,{"$f":"F357*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735001285"]
["TECHNIK","DN  0,34- 5 / 100",null,"Dutinka neizolovaná cínovaná, průřez 0,34mm2 / délka 5mm, dle DIN46228, (100ks)","100ks",0.81647498060871926,{"$f":"F358*(1-Elteq!$F$9)","v":0.81647498060871926},"8591735048570"]
["TECHNIK","DN  0,34- 7",null,"Dutinka neizolovaná cínovaná, průřez 0,34mm2 / délka 7mm, dle DIN46228","1000ks",7.6080623193085195,{"$f":"F359*(1-Elteq!$F$9)","v":7.6080623193085195},"8591735001292"]
["TECHNIK","DN  0,34- 7 / 100",null,"Dutinka neizolovaná cínovaná, průřez 0,34mm2 / délka 7mm, dle DIN46228, (100ks)","100ks",0.90925622840516462,{"$f":"F360*(1-Elteq!$F$9)","v":0.90925622840516462},"8591735033309"]
["TECHNIK","DN  0,5- 6",null,"Dutinka neizolovaná cínovaná, průřez 0,50mm2 / délka 6mm, dle DIN46228","1000ks",5.7895498624981911,{"$f":"F361*(1-Elteq!$F$9)","v":5.7895498624981911},"8591735001308"]
["TECHNIK","DN  0,5- 6 / 100",null,"Dutinka neizolovaná cínovaná, průřez 0,50mm2 / délka 6mm, dle DIN46228, (100ks)","100ks",0.76080623193085195,{"$f":"F362*(1-Elteq!$F$9)","v":0.76080623193085195},"8591735017477"]
["TECHNIK","DN  0,5- 8",null,"Dutinka neizolovaná cínovaná, průřez 0,50mm2 / délka 8mm, dle DIN46228","1000ks",7.274049827241317,{"$f":"F363*(1-Elteq!$F$9)","v":7.274049827241317},"8591735001315"]
["TECHNIK","DN  0,5- 8 / 100",null,"Dutinka neizolovaná cínovaná, průřez 0,50mm2 / délka 8mm, dle DIN46228, (100ks)","100ks",0.90925622840516462,{"$f":"F364*(1-Elteq!$F$9)","v":0.90925622840516462},"8591735030476"]
["TECHNIK","DN  0,5-10",null,"Dutinka neizolovaná cínovaná, průřez 0,50mm2 / délka 10mm, dle DIN46228","1000ks",8.090524807850036,{"$f":"F365*(1-Elteq!$F$9)","v":8.090524807850036},"8591735001322"]
["TECHNIK","DN  0,5-10 / 100",null,"Dutinka neizolovaná cínovaná, průřez 0,50mm2 / délka 10mm, dle DIN46228, (100ks)","100ks",1.00203747620161,{"$f":"F366*(1-Elteq!$F$9)","v":1.00203747620161},"8591735032524"]
["TECHNIK","DN  0,5-12",null,"Dutinka neizolovaná cínovaná, průřez 0,50mm2 / délka 12mm, dle DIN46228","1000ks",9.5750247725931619,{"$f":"F367*(1-Elteq!$F$9)","v":9.5750247725931619},"8591735002909"]
["TECHNIK","DN  0,5-12 / 100",null,"Dutinka neizolovaná cínovaná, průřez 0,50mm2 / délka 12mm, dle DIN46228, (100ks)","100ks",1.1504874726759224,{"$f":"F368*(1-Elteq!$F$9)","v":1.1504874726759224},"8591735036324"]
["TECHNIK","DN  0,75- 6",null,"Dutinka neizolovaná cínovaná, průřez 0,75mm2 / délka 6mm, dle DIN46228","1000ks",5.7895498624981911,{"$f":"F369*(1-Elteq!$F$9)","v":5.7895498624981911},"8591735001339"]
["TECHNIK","DN  0,75- 6 / 100",null,"Dutinka neizolovaná cínovaná, průřez 0,75mm2 / délka 6mm, dle DIN46228, (100ks)","100ks",0.76080623193085195,{"$f":"F370*(1-Elteq!$F$9)","v":0.76080623193085195},"8591735035419"]
["TECHNIK","DN  0,75- 8",null,"Dutinka neizolovaná cínovaná, průřez 0,75mm2 / délka 8mm, dle DIN46228","1000ks",7.274049827241317,{"$f":"F371*(1-Elteq!$F$9)","v":7.274049827241317},"8591735001346"]
["TECHNIK","DN  0,75- 8 / 100",null,"Dutinka neizolovaná cínovaná, průřez 0,75mm2 / délka 8mm, dle DIN46228, (100ks)","100ks",0.90925622840516462,{"$f":"F372*(1-Elteq!$F$9)","v":0.90925622840516462},"8591735018733"]
["TECHNIK","DN  0,75-10",null,"Dutinka neizolovaná cínovaná, průřez 0,75mm2 / délka 10mm, dle DIN46228","1000ks",8.1276373069686141,{"$f":"F373*(1-Elteq!$F$9)","v":8.1276373069686141},"8591735001353"]
["TECHNIK","DN  0,75-10 / 100",null,"Dutinka neizolovaná cínovaná, průřez 0,75mm2 / délka 10mm, dle DIN46228, (100ks)","100ks",1.00203747620161,{"$f":"F374*(1-Elteq!$F$9)","v":1.00203747620161},"8591735030483"]
["TECHNIK","DN  0,75-12",null,"Dutinka neizolovaná cínovaná, průřez 0,75mm2 / délka 12mm, dle DIN46228","1000ks",9.5750247725931619,{"$f":"F375*(1-Elteq!$F$9)","v":9.5750247725931619},"8591735002916"]
["TECHNIK","DN  0,75-15",null,"Dutinka neizolovaná cínovaná, průřez 0,75mm2 / délka 15mm, dle DIN46228","1000ks",11.39353722940349,{"$f":"F376*(1-Elteq!$F$9)","v":11.39353722940349},"8591735002923"]
["TECHNIK","DN  0,75-15 / 100",null,"Dutinka neizolovaná cínovaná, průřez 0,75mm2 / délka 15mm, dle DIN46228, (100ks)","100ks",1.3731624673873914,{"$f":"F377*(1-Elteq!$F$9)","v":1.3731624673873914},"8591735035365"]
["TECHNIK","DN  0,75-20",null,"Dutinka neizolovaná cínovaná, průřez 0,75mm2 / délka 20mm, dle DIN46228","1000ks",13.880074670348227,{"$f":"F378*(1-Elteq!$F$9)","v":13.880074670348227},"8591735033927"]
["TECHNIK","DN  1,0- 6",null,"Dutinka neizolovaná cínovaná, průřez 1,0mm2 / délka 6mm, dle DIN46228","1000ks",5.8637748607353473,{"$f":"F379*(1-Elteq!$F$9)","v":5.8637748607353473},"8591735001360"]
["TECHNIK","DN  1,0- 6 / 100",null,"Dutinka neizolovaná cínovaná, průřez 1,0mm2 / délka 6mm, dle DIN46228, (100ks)","100ks",0.76080623193085195,{"$f":"F380*(1-Elteq!$F$9)","v":0.76080623193085195},"8591735017576"]
["TECHNIK","DN  1,0- 8",null,"Dutinka neizolovaná cínovaná, průřez 1,0mm2 / délka 8mm, dle DIN46228","1000ks",7.274049827241317,{"$f":"F381*(1-Elteq!$F$9)","v":7.274049827241317},"8591735001377"]
["TECHNIK","DN  1,0- 8 / 100",null,"Dutinka neizolovaná cínovaná, průřez 1,0mm2 / délka 8mm, dle DIN46228, (100ks)","100ks",0.90925622840516462,{"$f":"F382*(1-Elteq!$F$9)","v":0.90925622840516462},"8591735030490"]
["TECHNIK","DN  1,0-10",null,"Dutinka neizolovaná cínovaná, průřez 1,0mm2 / délka 10mm, dle DIN46228","1000ks",8.3874248007986605,{"$f":"F383*(1-Elteq!$F$9)","v":8.3874248007986605},"8591735001384"]
["TECHNIK","DN  1,0-10 / 100",null,"Dutinka neizolovaná cínovaná, průřez 1,0mm2 / délka 10mm, dle DIN46228, (100ks)","100ks",1.00203747620161,{"$f":"F384*(1-Elteq!$F$9)","v":1.00203747620161},"8591735017828"]
["TECHNIK","DN  1,0-12",null,"Dutinka neizolovaná cínovaná, průřez 1,0mm2 / délka 12mm, dle DIN46228","1000ks",9.9090372646603644,{"$f":"F385*(1-Elteq!$F$9)","v":9.9090372646603644},"8591735001391"]
["TECHNIK","DN  1,0-12 / 100",null,"Dutinka neizolovaná cínovaná, průřez 1,0mm2 / délka 12mm, dle DIN46228, (100ks)","100ks",1.1875999717945007,{"$f":"F386*(1-Elteq!$F$9)","v":1.1875999717945007},"8591735054502"]
["TECHNIK","DN  1,0-15",null,"Dutinka neizolovaná cínovaná, průřez 1,0mm2 / délka 15mm, dle DIN46228","1000ks",11.39353722940349,{"$f":"F387*(1-Elteq!$F$9)","v":11.39353722940349},"8591735011154"]
["TECHNIK","DN  1,0-15 / 100",null,"Dutinka neizolovaná cínovaná, průřez 1,0mm2 / délka 15mm, dle DIN46228, (100ks)","100ks",1.3731624673873914,{"$f":"F388*(1-Elteq!$F$9)","v":1.3731624673873914},"8591735036317"]
["TECHNIK","DN  1,0-18",null,"Dutinka neizolovaná cínovaná, průřez 1,0mm2 / délka 18mm, dle DIN46228","1000ks",15.587249629802821,{"$f":"F389*(1-Elteq!$F$9)","v":15.587249629802821},"8591735011161"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"DN  1,0-20",null,"Dutinka neizolovaná cínovaná, průřez 1,0mm2 / délka 20mm, dle DIN46228","1000ks",16.552174606885853,{"$f":"F390*(1-Elteq!$F$9)","v":16.552174606885853},"8591735033934"]
["TECHNIK","DN  1,5- 6",null,"Dutinka neizolovaná cínovaná, průřez 1,5mm2 / délka 6mm, dle DIN46228","1000ks",5.8637748607353473,{"$f":"F391*(1-Elteq!$F$9)","v":5.8637748607353473},"8591735001407"]
["TECHNIK","DN  1,5- 6 / 100",null,"Dutinka neizolovaná cínovaná, průřez 1,5mm2 / délka 6mm, dle DIN46228, (100ks)","100ks",0.76080623193085195,{"$f":"F392*(1-Elteq!$F$9)","v":0.76080623193085195},"8591735017491"]
["TECHNIK","DN  1,5- 7",null,"Dutinka neizolovaná cínovaná, průřez 1,5mm2 / délka 7mm, dle DIN46228","1000ks",7.0513748325298478,{"$f":"F393*(1-Elteq!$F$9)","v":7.0513748325298478},"8591735001414"]
["TECHNIK","DN  1,5- 8",null,"Dutinka neizolovaná cínovaná, průřez 1,5mm2 / délka 8mm, dle DIN46228","1000ks",7.274049827241317,{"$f":"F394*(1-Elteq!$F$9)","v":7.274049827241317},"8591735001421"]
["TECHNIK","DN  1,5- 8 / 100",null,"Dutinka neizolovaná cínovaná, průřez 1,5mm2 / délka 8mm, dle DIN46228, (100ks)","100ks",0.90925622840516462,{"$f":"F395*(1-Elteq!$F$9)","v":0.90925622840516462},"8591735017484"]
["TECHNIK","DN  1,5-10",null,"Dutinka neizolovaná cínovaná, průřez 1,5mm2 / délka 10mm, dle DIN46228","1000ks",8.6472122946287087,{"$f":"F396*(1-Elteq!$F$9)","v":8.6472122946287087},"8591735001438"]
["TECHNIK","DN  1,5-10 / 100",null,"Dutinka neizolovaná cínovaná, průřez 1,5mm2 / délka 10mm, dle DIN46228, (100ks)","100ks",1.00203747620161,{"$f":"F397*(1-Elteq!$F$9)","v":1.00203747620161},"8591735017835"]
["TECHNIK","DN  1,5-12",null,"Dutinka neizolovaná cínovaná, průřez 1,5mm2 / délka 12mm, dle DIN46228","1000ks",10.539949749676193,{"$f":"F398*(1-Elteq!$F$9)","v":10.539949749676193},"8591735001445"]
["TECHNIK","DN  1,5-12 / 100",null,"Dutinka neizolovaná cínovaná, průřez 1,5mm2 / délka 12mm, dle DIN46228, (100ks)","100ks",1.2618249700316571,{"$f":"F399*(1-Elteq!$F$9)","v":1.2618249700316571},"8591735054519"]
["TECHNIK","DN  1,5-15",null,"Dutinka neizolovaná cínovaná, průřez 1,5mm2 / délka 15mm, dle DIN46228","1000ks",12.581137201197992,{"$f":"F400*(1-Elteq!$F$9)","v":12.581137201197992},"8591735011178"]
["TECHNIK","DN  1,5-15 / 100",null,"Dutinka neizolovaná cínovaná, průřez 1,5mm2 / délka 15mm, dle DIN46228, (100ks)","100ks",1.4844999647431258,{"$f":"F401*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735035402"]
["TECHNIK","DN  1,5-18",null,"Dutinka neizolovaná cínovaná, průřez 1,5mm2 / délka 18mm, dle DIN46228","1000ks",14.696549650956946,{"$f":"F402*(1-Elteq!$F$9)","v":14.696549650956946},"8591735001452"]
["TECHNIK","DN  1,5-20",null,"Dutinka neizolovaná cínovaná, průřez 1,5mm2 / délka 20mm, dle DIN46228","1000ks",16.106824617462916,{"$f":"F403*(1-Elteq!$F$9)","v":16.106824617462916},"8591735030971"]
["TECHNIK","DN  2,5- 7",null,"Dutinka neizolovaná cínovaná, průřez 2,5mm2 / délka 7mm, dle DIN46228","1000ks",7.7936248149014107,{"$f":"F404*(1-Elteq!$F$9)","v":7.7936248149014107},"8591735001469"]
["TECHNIK","DN  2,5- 7 / 100",null,"Dutinka neizolovaná cínovaná, průřez 2,5mm2 / délka 7mm, dle DIN46228, (100ks)","100ks",0.96492497708303182,{"$f":"F405*(1-Elteq!$F$9)","v":0.96492497708303182},"8591735030506"]
["TECHNIK","DN  2,5- 8",null,"Dutinka neizolovaná cínovaná, průřez 2,5mm2 / délka 8mm, dle DIN46228","1000ks",9.7605872681860522,{"$f":"F406*(1-Elteq!$F$9)","v":9.7605872681860522},"8591735018177"]
["TECHNIK","DN  2,5- 8 / 100",null,"Dutinka neizolovaná cínovaná, průřez 2,5mm2 / délka 8mm, dle DIN46228, (100ks)","100ks",1.1504874726759224,{"$f":"F407*(1-Elteq!$F$9)","v":1.1504874726759224},"8591735030513"]
["TECHNIK","DN  2,5-10",null,"Dutinka neizolovaná cínovaná, průřez 2,5mm2 / délka 10mm, dle DIN46228","1000ks",10.762624744387661,{"$f":"F408*(1-Elteq!$F$9)","v":10.762624744387661},"8591735001476"]
["TECHNIK","DN  2,5-10 / 100",null,"Dutinka neizolovaná cínovaná, průřez 2,5mm2 / délka 10mm, dle DIN46228, (100ks)","100ks",1.2618249700316571,{"$f":"F409*(1-Elteq!$F$9)","v":1.2618249700316571},"8591735030520"]
["TECHNIK","DN  2,5-12",null,"Dutinka neizolovaná cínovaná, průřez 2,5mm2 / délka 12mm, dle DIN46228","1000ks",11.950224716182163,{"$f":"F410*(1-Elteq!$F$9)","v":11.950224716182163},"8591735001483"]
["TECHNIK","DN  2,5-12 / 100",null,"Dutinka neizolovaná cínovaná, průřez 2,5mm2 / délka 12mm, dle DIN46228, (100ks)","100ks",1.3731624673873914,{"$f":"F411*(1-Elteq!$F$9)","v":1.3731624673873914},"8591735035372"]
["TECHNIK","DN  2,5-15",null,"Dutinka neizolovaná cínovaná, průřez 2,5mm2 / délka 15mm, dle DIN46228","1000ks",14.473874656245476,{"$f":"F412*(1-Elteq!$F$9)","v":14.473874656245476},"8591735011192"]
["TECHNIK","DN  2,5-18",null,"Dutinka neizolovaná cínovaná, průřez 2,5mm2 / délka 18mm, dle DIN46228","1000ks",16.589287106004431,{"$f":"F413*(1-Elteq!$F$9)","v":16.589287106004431},"8591735001490"]
["TECHNIK","DN  2,5-18 / 100",null,"Dutinka neizolovaná cínovaná, průřez 2,5mm2 / délka 18mm, dle DIN46228, (100ks)","100ks",1.9669624532846417,{"$f":"F414*(1-Elteq!$F$9)","v":1.9669624532846417},"8591735035396"]
["TECHNIK","DN  2,5-20",null,"Dutinka neizolovaná cínovaná, průřez 2,5mm2 / délka 20mm, dle DIN46228","1000ks",18.370687063696181,{"$f":"F415*(1-Elteq!$F$9)","v":18.370687063696181},"8591735030988"]
["TECHNIK","DN  2,5-25",null,"Dutinka neizolovaná cínovaná, průřez 2,5mm2 / délka 25mm, dle DIN46228","1000ks",25.199386901514561,{"$f":"F416*(1-Elteq!$F$9)","v":25.199386901514561},"8591735033941"]
["TECHNIK","DN  4- 9",null,"Dutinka neizolovaná cínovaná, průřez 4,0mm2 / délka 9mm, dle DIN46228","500ks",6.0493373563282375,{"$f":"F417*(1-Elteq!$F$9)","v":6.0493373563282375},"8591735001506"]
["TECHNIK","DN  4- 9 / 100",null,"Dutinka neizolovaná cínovaná, průřez 4,0mm2 / délka 9mm, dle DIN46228, (100ks)","100ks",1.2618249700316571,{"$f":"F418*(1-Elteq!$F$9)","v":1.2618249700316571},"8591735030537"]
["TECHNIK","DN  4-10",null,"Dutinka neizolovaná cínovaná, průřez 4,0mm2 / délka 10mm, dle DIN46228","500ks",7.0884873316484258,{"$f":"F419*(1-Elteq!$F$9)","v":7.0884873316484258},"8591735026981"]
["TECHNIK","DN  4-10 / 100",null,"Dutinka neizolovaná cínovaná, průřez 4,0mm2 / délka 10mm, dle DIN46228, (100ks)","100ks",1.5216124638617039,{"$f":"F420*(1-Elteq!$F$9)","v":1.5216124638617039},"8591735035549"]
["TECHNIK","DN  4-12",null,"Dutinka neizolovaná cínovaná, průřez 4,0mm2 / délka 12mm, dle DIN46228","500ks",7.4596123228342073,{"$f":"F421*(1-Elteq!$F$9)","v":7.4596123228342073},"8591735001513"]
["TECHNIK","DN  4-12 / 100",null,"Dutinka neizolovaná cínovaná, průřez 4,0mm2 / délka 12mm, dle DIN46228, (100ks)","100ks",1.6329499612174385,{"$f":"F422*(1-Elteq!$F$9)","v":1.6329499612174385},"8591735033347"]
["TECHNIK","DN  4-15",null,"Dutinka neizolovaná cínovaná, průřez 4,0mm2 / délka 15mm, dle DIN46228","500ks",9.0925622840516453,{"$f":"F423*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735001520"]
["TECHNIK","DN  4-18",null,"Dutinka neizolovaná cínovaná, průřez 4,0mm2 / délka 18mm, dle DIN46228","500ks",9.5750247725931619,{"$f":"F424*(1-Elteq!$F$9)","v":9.5750247725931619},"8591735001537"]
["TECHNIK","DN  4-18 / 100",null,"Dutinka neizolovaná cínovaná, průřez 4,0mm2 / délka 18mm, dle DIN46228, (100ks)","100ks",2.041187451521798,{"$f":"F425*(1-Elteq!$F$9)","v":2.041187451521798},"8591735035389"]
["TECHNIK","DN  4-20",null,"Dutinka neizolovaná cínovaná, průřez 4,0mm2 / délka 20mm, dle DIN46228","500ks",11.950224716182163,{"$f":"F426*(1-Elteq!$F$9)","v":11.950224716182163},"8591735024642"]
["TECHNIK","DN  6- 6",null,"Dutinka neizolovaná cínovaná, průřez 6,0mm2 / délka 6mm, dle DIN46228","250ks",3.5627999153835019,{"$f":"F427*(1-Elteq!$F$9)","v":3.5627999153835019},"8591735033958"]
["TECHNIK","DN  6-10",null,"Dutinka neizolovaná cínovaná, průřez 6,0mm2 / délka 10mm, dle DIN46228","250ks",3.4885749171463458,{"$f":"F428*(1-Elteq!$F$9)","v":3.4885749171463458},"8591735011024"]
["TECHNIK","DN  6-10 / 100",null,"Dutinka neizolovaná cínovaná, průřez 6,0mm2 / délka 10mm, dle DIN46228, (100ks)","100ks",1.4473874656245478,{"$f":"F429*(1-Elteq!$F$9)","v":1.4473874656245478},"8591735030544"]
["TECHNIK","DN  6-12",null,"Dutinka neizolovaná cínovaná, průřez 6,0mm2 / délka 12mm, dle DIN46228","250ks",4.5648373915851117,{"$f":"F430*(1-Elteq!$F$9)","v":4.5648373915851117},"8591735001551"]
["TECHNIK","DN  6-12 / 100",null,"Dutinka neizolovaná cínovaná, průřez 6,0mm2 / délka 12mm, dle DIN46228, (100ks)","100ks",1.8927374550474854,{"$f":"F431*(1-Elteq!$F$9)","v":1.8927374550474854},"8591735017712"]
["TECHNIK","DN  6-15",null,"Dutinka neizolovaná cínovaná, průřez 6,0mm2 / délka 15mm, dle DIN46228","100ks",2.0782999506403761,{"$f":"F432*(1-Elteq!$F$9)","v":2.0782999506403761},"8591735001568"]
["TECHNIK","DN  6-18",null,"Dutinka neizolovaná cínovaná, průřez 6,0mm2 / délka 18mm, dle DIN46228","250ks",5.5668748677867219,{"$f":"F433*(1-Elteq!$F$9)","v":5.5668748677867219},"8591735038533"]
["TECHNIK","DN  6-18 / 100",null,"Dutinka neizolovaná cínovaná, průřez 6,0mm2 / délka 18mm, dle DIN46228, (100ks)","100ks",2.2638624462332668,{"$f":"F434*(1-Elteq!$F$9)","v":2.2638624462332668},"8591735001575"]
["TECHNIK","DN  6-20",null,"Dutinka neizolovaná cínovaná, průřez 6,0mm2 / délka 20mm, dle DIN46228","100ks",2.5978749383004702,{"$f":"F435*(1-Elteq!$F$9)","v":2.5978749383004702},"8591735024659"]
["TECHNIK","DN 10-12",null,"Dutinka neizolovaná cínovaná, průřez 10mm2 / délka 12mm, dle DIN46228","250ks",4.824624885415159,{"$f":"F436*(1-Elteq!$F$9)","v":4.824624885415159},"8591735033194"]
["TECHNIK","DN 10-12 / 100",null,"Dutinka neizolovaná cínovaná, průřez 10mm2 / délka 12mm, dle DIN46228, (100ks)","100ks",1.9669624532846417,{"$f":"F437*(1-Elteq!$F$9)","v":1.9669624532846417},"8591735001582"]
["TECHNIK","DN 10-15",null,"Dutinka neizolovaná cínovaná, průřez 10mm2 / délka 15 mm, dle DIN46228","100ks",2.3751999435890014,{"$f":"F438*(1-Elteq!$F$9)","v":2.3751999435890014},"8591735001599"]
["TECHNIK","DN 10-18",null,"Dutinka neizolovaná cínovaná, průřez 10mm2 / délka 18 mm, dle DIN46228","100ks",2.5978749383004702,{"$f":"F439*(1-Elteq!$F$9)","v":2.5978749383004702},"8591735001605"]
["TECHNIK","DN 10-20",null,"Dutinka neizolovaná cínovaná, průřez 10mm2 / délka 20 mm, dle DIN46228","100ks",2.8576624321305171,{"$f":"F440*(1-Elteq!$F$9)","v":2.8576624321305171},"8591735024666"]
["TECHNIK","DN 10-25",null,"Dutinka neizolovaná cínovaná, průřez 10mm2 / délka 25 mm, dle DIN46228","100ks",3.3030124215534551,{"$f":"F441*(1-Elteq!$F$9)","v":3.3030124215534551},"8591735011208"]
["TECHNIK","DN 16-12",null,"Dutinka neizolovaná cínovaná, průřez 16mm2 / délka 12mm, dle DIN46228","100ks",2.5978749383004702,{"$f":"F442*(1-Elteq!$F$9)","v":2.5978749383004702},"8591735001612"]
["TECHNIK","DN 16-15",null,"Dutinka neizolovaná cínovaná, průřez 16mm2 / délka 15mm, dle DIN46228","100ks",3.4143499189091893,{"$f":"F443*(1-Elteq!$F$9)","v":3.4143499189091893},"8591735001629"]
["TECHNIK","DN 16-18",null,"Dutinka neizolovaná cínovaná, průřez 16mm2 / délka 18mm, dle DIN46228","100ks",3.5627999153835019,{"$f":"F444*(1-Elteq!$F$9)","v":3.5627999153835019},"8591735001636"]
["TECHNIK","DN 16-20",null,"Dutinka neizolovaná cínovaná, průřez 16mm2 / délka 20mm, dle DIN46228","100ks",4.3421623968736434,{"$f":"F445*(1-Elteq!$F$9)","v":4.3421623968736434},"8591735024673"]
["TECHNIK","DN 16-25",null,"Dutinka neizolovaná cínovaná, průřez 16mm2 / délka 25mm, dle DIN46228","100ks",4.824624885415159,{"$f":"F446*(1-Elteq!$F$9)","v":4.824624885415159},"8591735011215"]
["TECHNIK","DN 16-32",null,"Dutinka neizolovaná cínovaná, průřez 16mm2 / délka 32mm, dle DIN46228","100ks",5.1586373774823624,{"$f":"F447*(1-Elteq!$F$9)","v":5.1586373774823624},"8591735011222"]
["TECHNIK","DN 25-12",null,"Dutinka neizolovaná cínovaná, průřez 25mm2 / délka 12mm, dle DIN46228","50ks",2.1154124497589541,{"$f":"F448*(1-Elteq!$F$9)","v":2.1154124497589541},"8591735001643"]
["TECHNIK","DN 25-15",null,"Dutinka neizolovaná cínovaná, průřez 25mm2 / délka 15mm, dle DIN46228","50ks",2.5978749383004702,{"$f":"F449*(1-Elteq!$F$9)","v":2.5978749383004702},"8591735001650"]
["TECHNIK","DN 25-18",null,"Dutinka neizolovaná cínovaná, průřez 25mm2 / délka 18mm, dle DIN46228","50ks",2.820549933011939,{"$f":"F450*(1-Elteq!$F$9)","v":2.820549933011939},"8591735001667"]
["TECHNIK","DN 25-25",null,"Dutinka neizolovaná cínovaná, průřez 25mm2 / délka 25mm, dle DIN46228","50ks",3.6370249136206585,{"$f":"F451*(1-Elteq!$F$9)","v":3.6370249136206585},"8591735011239"]
["TECHNIK","DN 25-32",null,"Dutinka neizolovaná cínovaná, průřez 25mm2 / délka 32mm, dle DIN46228","50ks",4.00814990480644,{"$f":"F452*(1-Elteq!$F$9)","v":4.00814990480644},"8591735011246"]
["TECHNIK","DN 35-12",null,"Dutinka neizolovaná cínovaná, průřez 35mm2 / délka 12mm, dle DIN46228","100ks",4.1194874021621741,{"$f":"F453*(1-Elteq!$F$9)","v":4.1194874021621741},"8591735001674"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"DN 35-15",null,"Dutinka neizolovaná cínovaná, průřez 35mm2 / délka 15mm, dle DIN46228","50ks",2.820549933011939,{"$f":"F454*(1-Elteq!$F$9)","v":2.820549933011939},"8591735011253"]
["TECHNIK","DN 35-18",null,"Dutinka neizolovaná cínovaná, průřez 35mm2 / délka 18mm, dle DIN46228","50ks",2.8947749312490956,{"$f":"F455*(1-Elteq!$F$9)","v":2.8947749312490956},"8591735001681"]
["TECHNIK","DN 35-20",null,"Dutinka neizolovaná cínovaná, průřez 35mm2 / délka 20mm, dle DIN46228","50ks",3.7112499118578146,{"$f":"F456*(1-Elteq!$F$9)","v":3.7112499118578146},"8591735026707"]
["TECHNIK","DN 35-25",null,"Dutinka neizolovaná cínovaná, průřez 35mm2 / délka 25mm, dle DIN46228","50ks",3.9710374056878615,{"$f":"F457*(1-Elteq!$F$9)","v":3.9710374056878615},"8591735001698"]
["TECHNIK","DN 35-32",null,"Dutinka neizolovaná cínovaná, průřez 35mm2 / délka 32mm, dle DIN46228","50ks",4.7503998871780029,{"$f":"F458*(1-Elteq!$F$9)","v":4.7503998871780029},"8591735011260"]
["TECHNIK","DN 50-12",null,"Dutinka neizolovaná cínovaná, průřez 50mm2 / délka 12mm, dle DIN46228","50ks",5.7153248642610341,{"$f":"F459*(1-Elteq!$F$9)","v":5.7153248642610341},"8591735034962"]
["TECHNIK","DN 50-18",null,"Dutinka neizolovaná cínovaná, průřez 50mm2 / délka 18mm, dle DIN46228","50ks",5.5668748677867219,{"$f":"F460*(1-Elteq!$F$9)","v":5.5668748677867219},"8591735001704"]
["TECHNIK","DN 50-22",null,"Dutinka neizolovaná cínovaná, průřez 50mm2 / délka 22mm, dle DIN46228","50ks",8.2389748043243483,{"$f":"F461*(1-Elteq!$F$9)","v":8.2389748043243483},"8591735011277"]
["TECHNIK","DN 50-25",null,"Dutinka neizolovaná cínovaná, průřez 50mm2 / délka 25mm, dle DIN46228","50ks",8.5358747972729727,{"$f":"F462*(1-Elteq!$F$9)","v":8.5358747972729727},"8591735026714"]
["TECHNIK","DN 50-32",null,"Dutinka neizolovaná cínovaná, průřez 50mm2 / délka 32mm, dle DIN46228","50ks",9.8719247655417863,{"$f":"F463*(1-Elteq!$F$9)","v":9.8719247655417863},"8591735011284"]
["TECHNIK","DN 70-25",null,"Dutinka neizolovaná cínovaná, průřez 70mm2 / délka 25mm, dle DIN46228","50ks",12.395574705605101,{"$f":"F464*(1-Elteq!$F$9)","v":12.395574705605101},"8591735001711"]
["TECHNIK","DN 70-32",null,"Dutinka neizolovaná cínovaná, průřez 70mm2 / délka 32mm, dle DIN46228","50ks",14.473874656245476,{"$f":"F465*(1-Elteq!$F$9)","v":14.473874656245476},"8591735011291"]
["TECHNIK","DN 95-25",null,"Dutinka neizolovaná cínovaná, průřez 95mm2 / délka 25mm, dle DIN46228","50ks",14.510987155364054,{"$f":"F466*(1-Elteq!$F$9)","v":14.510987155364054},"8591735001728"]
["TECHNIK","DN 95-32",null,"Dutinka neizolovaná cínovaná, průřez 95mm2 / délka 32mm, dle DIN46228","50ks",16.03259961922576,{"$f":"F467*(1-Elteq!$F$9)","v":16.03259961922576},"8591735011307"]
["TECHNIK","DN120-32",null,"Dutinka neizolovaná cínovaná, průřez 120mm2 / délka 32mm, dle DIN46228","25ks",12.172899710893631,{"$f":"F468*(1-Elteq!$F$9)","v":12.172899710893631},"8591735001735"]
["TECHNIK","DN120-38",null,"Dutinka neizolovaná cínovaná, průřez 120mm2 / délka 38mm, dle DIN46228","25ks",14.993449643905571,{"$f":"F469*(1-Elteq!$F$9)","v":14.993449643905571},"8591735033965"]
["TECHNIK","DN150-32",null,"Dutinka neizolovaná cínovaná, průřez 150mm2 / délka 32mm, dle DIN46228","25ks",12.766699696790882,{"$f":"F470*(1-Elteq!$F$9)","v":12.766699696790882},"8591735001742"]
["TECHNIK","DN150-38",null,"Dutinka neizolovaná cínovaná, průřez 150mm2 / délka 38mm, dle DIN46228","25ks",14.993449643905571,{"$f":"F471*(1-Elteq!$F$9)","v":14.993449643905571},"8591735026691"]
["TECHNIK","DN185-32",null,"Dutinka neizolovaná cínovaná, průřez 185mm2 / délka 32mm, dle DIN46228","25ks",16.700624603360165,{"$f":"F472*(1-Elteq!$F$9)","v":16.700624603360165},"8591735001759"]
["TECHNIK","DN185-40",null,"Dutinka neizolovaná cínovaná, průřez 185mm2 / délka 40mm, dle DIN46228","25ks",19.001599548712012,{"$f":"F473*(1-Elteq!$F$9)","v":19.001599548712012},"8591735015664"]
["TECHNIK","DN240-40",null,"Dutinka neizolovaná cínovaná, průřez 240mm2 / délka 40mm, dle DIN46228","25ks",34.514624180277679,{"$f":"F474*(1-Elteq!$F$9)","v":34.514624180277679},"8591735018528"]
["TECHNIK","PBOX černý",null,"Plastový box na dutinky 5-dílný bez potisku, barva černá","1ks",4.0823749030435961,{"$f":"F475*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735050023"]
["TECHNIK","PBOX modrý",null,"Plastový box na dutinky 5-dílný bez potisku, barva modrá","1ks",4.0823749030435961,{"$f":"F476*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735050054"]
["TECHNIK","PBOX oranžový",null,"Plastový box na dutinky 5-dílný bez potisku, barva oranžová","1ks",4.0823749030435961,{"$f":"F477*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735050078"]
["TECHNIK","PBOX rudý",null,"Plastový box na dutinky 5-dílný bez potisku, barva červená","1ks",4.0823749030435961,{"$f":"F478*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735050085"]
["TECHNIK","PBOX sv. šedý",null,"Plastový box na dutinky 5-dílný bez potisku, barva světle šedá","1ks",4.0823749030435961,{"$f":"F479*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735050047"]
["TECHNIK","PBOX tm. šedý",null,"Plastový box na dutinky 5-dílný bez potisku, barva tmavě šedá","1ks",4.0823749030435961,{"$f":"F480*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735050030"]
["TECHNIK","PBOX zelený",null,"Plastový box na dutinky 5-dílný bez potisku, barva zelená","1ks",4.0823749030435961,{"$f":"F481*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735050061"]
["TECHNIK","PBOX žlutý",null,"Plastový box na dutinky 5-dílný bez potisku, barva žlutá","1ks",4.0823749030435961,{"$f":"F482*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735050092"]
["TECHNIK","PD 1",null,"Dóza 1-dílná prázdná bez potisku pro libovolné průřezy","1ks",4.3050498977550653,{"$f":"F483*(1-Elteq!$F$9)","v":4.3050498977550653},"8591735010836"]
["TECHNIK","PD 4",null,"Dóza 4-dílná prázdná s potiskem pro průřezy 4,0-16mm2","1ks",2.9318874303676736,{"$f":"F484*(1-Elteq!$F$9)","v":2.9318874303676736},"8591735001766"]
["TECHNIK","PD 4N",null,"Dóza 4-dílná prázdná bez potisku pro libovolné průřezy","1ks",2.9318874303676736,{"$f":"F485*(1-Elteq!$F$9)","v":2.9318874303676736},"8591735030995"]
["TECHNIK","PD 5",null,"Dóza 5-dílná prázdná s potiskem pro průřezy 0,5-2,5mm2","1ks",2.9318874303676736,{"$f":"F486*(1-Elteq!$F$9)","v":2.9318874303676736},"8591735001773"]
["TECHNIK","PD 5N",null,"Dóza 5-dílná prázdná bez potisku pro libovolné průřezy","1ks",2.9318874303676736,{"$f":"F487*(1-Elteq!$F$9)","v":2.9318874303676736},"8591735031008"]
["TECHNIK","PDD 0525/1",null,"Dóza s dutinkami dvojitými, průřezy 0,5-2,5mm2, barevný kód 1","1ks",11.059524737336288,{"$f":"F488*(1-Elteq!$F$9)","v":11.059524737336288},"8591735001780"]
["TECHNIK","PDD 0525/2",null,"Dóza s dutinkami dvojitými, průřezy 0,5-2,5mm2, barevný kód 2","1ks",11.059524737336288,{"$f":"F489*(1-Elteq!$F$9)","v":11.059524737336288},"8591735031015"]
["TECHNIK","PDD 0525/3",null,"Dóza s dutinkami dvojitými, průřezy 0,5-2,5mm2, barevný kód 3","1ks",11.059524737336288,{"$f":"F490*(1-Elteq!$F$9)","v":11.059524737336288},"8591735013141"]
["TECHNIK","PDI 0,5- 8 oranžová",null,"Dóza s dutinkami izolovanými, průřez 0,50mm2 / délka 8mm","1ks",11.504874726759224,{"$f":"F491*(1-Elteq!$F$9)","v":11.504874726759224},"8591735031022"]
["TECHNIK","PDI 0,75- 8 bílá",null,"Dóza s dutinkami izolovanými, průřez 0,75mm2 / délka 8mm","1ks",11.504874726759224,{"$f":"F492*(1-Elteq!$F$9)","v":11.504874726759224},"8591735031039"]
["TECHNIK","PDI 0,75-10 bílá",null,"Dóza s dutinkami izolovanými, průřez 0,75mm2 / délka 10mm","1ks",17.44287458573173,{"$f":"F493*(1-Elteq!$F$9)","v":17.44287458573173},"8591735014179"]
["TECHNIK","PDI 0525/1",null,"Dóza s dutinkami izolovanými 0,5-2,5mm2, barebný kód 1","1ks",8.1276373069686141,{"$f":"F494*(1-Elteq!$F$9)","v":8.1276373069686141},"8591735001797"]
["TECHNIK","PDI 0525/2",null,"Dóza s dutinkami izolovanými 0,5-2,5mm2, barevný kód 2","1ks",8.1276373069686141,{"$f":"F495*(1-Elteq!$F$9)","v":8.1276373069686141},"8591735012656"]
["TECHNIK","PDI 0525/3",null,"Dóza s dutinkami izolovanými 0,5-2,5mm2, barevný kód 3","1ks",8.1276373069686141,{"$f":"F496*(1-Elteq!$F$9)","v":8.1276373069686141},"8591735014063"]
["TECHNIK","PDI 1- 8 žlutá",null,"Dóza s dutinkami izolovanými, průřez 1,0mm2 / délka 8mm","1ks",11.504874726759224,{"$f":"F497*(1-Elteq!$F$9)","v":11.504874726759224},"8591735010676"]
["TECHNIK","PDI 1,5- 8 rudá",null,"Dóza s dutinkami izolovanými, průřez 1,5mm2 / délka 8mm","1ks",11.504874726759224,{"$f":"F498*(1-Elteq!$F$9)","v":11.504874726759224},"8591735031046"]
["TECHNIK","PDI 1,5-10 rudá",null,"Dóza s dutinkami izolovanými, průřez 1,5mm2 / délka 10mm","1ks",17.44287458573173,{"$f":"F499*(1-Elteq!$F$9)","v":17.44287458573173},"8591735031053"]
["TECHNIK","PDI 1-10 žlutá",null,"Dóza s dutinkami izolovanými, průřez 1,0mm2 / délka 10mm","1ks",17.44287458573173,{"$f":"F500*(1-Elteq!$F$9)","v":17.44287458573173},"8591735017354"]
["TECHNIK","PDI 1-6/1",null,"Dóza s dutinkami izolovanými 1,0-6,0mm2, barevný kód 1","1ks",8.9812247866959112,{"$f":"F501*(1-Elteq!$F$9)","v":8.9812247866959112},"8591735024949"]
["TECHNIK","PDI 1-6/2",null,"Dóza s dutinkami izolovanými 1,0-6,0mm2, barevný kód 2","1ks",8.9812247866959112,{"$f":"F502*(1-Elteq!$F$9)","v":8.9812247866959112},"8591735031060"]
["TECHNIK","PDI 1-6/3",null,"Dóza s dutinkami izolovanými 1,0-6,0mm2, barevný kód 3","1ks",8.9812247866959112,{"$f":"F503*(1-Elteq!$F$9)","v":8.9812247866959112},"8591735029166"]
["TECHNIK","PDI 2,5- 8 modrá",null,"Dóza s dutinkami izolovanými, průřez 2,5mm2 / délka 8mm","1ks",12.692474698553726,{"$f":"F504*(1-Elteq!$F$9)","v":12.692474698553726},"8591735031077"]
["TECHNIK","PDI 4-10 šedá",null,"Dóza s dutinkami izolovanými, průřez 4,0mm2 / délka 10mm","1ks",11.950224716182163,{"$f":"F505*(1-Elteq!$F$9)","v":11.950224716182163},"8591735031084"]
["TECHNIK","PDI 416/1",null,"Dóza s dutinkami izolovanými 4-16mm2, barevný kód 1","1ks",6.6802498413440663,{"$f":"F506*(1-Elteq!$F$9)","v":6.6802498413440663},"8591735001803"]
["TECHNIK","PDI 416/2",null,"Dóza s dutinkami izolovanými 4-16mm2, barevný kód 2","1ks",6.6802498413440663,{"$f":"F507*(1-Elteq!$F$9)","v":6.6802498413440663},"8591735017552"]
["TECHNIK","PDI 416/3",null,"Dóza s dutinkami izolovanými 4-16mm2, barevný kód 3","1ks",6.6802498413440663,{"$f":"F508*(1-Elteq!$F$9)","v":6.6802498413440663},"8591735012663"]
["TECHNIK","PDI 6-12 černá",null,"Dóza s dutinkami izolovanými, průřez 6,0mm2 / délka 12mm","1ks",15.587249629802821,{"$f":"F509*(1-Elteq!$F$9)","v":15.587249629802821},"8591735031091"]
["TECHNIK","PDN 0525/6",null,"Dóza s dutinkami neizolovanými 0,5-2,5mm2 / délky 6mm","1ks",19.818074529320729,{"$f":"F510*(1-Elteq!$F$9)","v":19.818074529320729},"8591735001810"]
["TECHNIK","PDN 0525/8",null,"Dóza s dutinkami neizolovanými 0,5-2,5mm2 / délky 8mm","1ks",20.671662009048028,{"$f":"F511*(1-Elteq!$F$9)","v":20.671662009048028},"8591735001827"]
["TECHNIK","PDN 416",null,"Dóza s dutinkami neizolovanými 4-16mm2 / délky 9-12mm","1ks",10.131712259371835,{"$f":"F512*(1-Elteq!$F$9)","v":10.131712259371835},"8591735001834"]
["TECHNIK","KI 0,5- 8/PA",null,"Kolík izolovaný, průřez 0,1-0,5mm2 / délka 8mm, izolace PA","100ks",6.6802498413440663,{"$f":"F513*(1-Elteq!$F$9)","v":6.6802498413440663},"8591735015916"]
["TECHNIK","KI 0,5-10",null,"Kolík izolovaný, průřez 0,2-0,5mm2 / délka 10mm, izolace PVC","100ks",4.4906123933479556,{"$f":"F514*(1-Elteq!$F$9)","v":4.4906123933479556},"8591735031947"]
["TECHNIK","KI 1,5- 8",null,"Kolík izolovaný, průřez 0,5-1,5mm2 / délka 8mm, průměr špičky 1,9mm izolace PVC","100ks",4.824624885415159,{"$f":"F515*(1-Elteq!$F$9)","v":4.824624885415159},"8591735003517"]
["TECHNIK","KI 1,5- 8/E",null,"Kolík izolovaný, průřez 0,5-1,5mm2 / délka 8mm, průměr špičky 1,6mm izolace PVC s trychtýřem","100ks",5.1586373774823624,{"$f":"F516*(1-Elteq!$F$9)","v":5.1586373774823624},"8591735051860"]
["TECHNIK","KI 1,5- 8/PA",null,"Kolík izolovaný, průřez 0,5-1,5mm2 / délka 8mm, průměr špičky 1,9mm izolace PA s trychtýřem","100ks",5.8266623616167692,{"$f":"F517*(1-Elteq!$F$9)","v":5.8266623616167692},"8591735025502"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"KI 1,5- 8/PC",null,"Kolík izolovaný, průřez 0,5-1,5mm2 / délka 8mm, průměr špičky 1,9mm izolace PC s trychtýřem","100ks",5.9751123580910814,{"$f":"F518*(1-Elteq!$F$9)","v":5.9751123580910814},"8591735011734"]
["TECHNIK","KI 1,5-10",null,"Kolík izolovaný, průřez 0,5-1,5mm2 / délka 10mm, průměr špičky 1,9mm izolace PVC","100ks",5.0101873810080493,{"$f":"F519*(1-Elteq!$F$9)","v":5.0101873810080493},"8591735003524"]
["TECHNIK","KI 1,5-10/E",null,"Kolík izolovaný, průřez 0,5-1,5mm2 / délka 10mm, průměr špičky 1,9mm izolace PVC s trychtýřem","100ks",5.2699748748380966,{"$f":"F520*(1-Elteq!$F$9)","v":5.2699748748380966},"8591735027179"]
["TECHNIK","KI 1,5-10/PA",null,"Kolík izolovaný, průřez 0,5-1,5mm2 / délka 10mm, průměr špičky 1,9mm izolace PA s trychtýřem","100ks",5.9008873598539253,{"$f":"F521*(1-Elteq!$F$9)","v":5.9008873598539253},"8591735034030"]
["TECHNIK","KI 1,5-10/PC",null,"Kolík izolovaný, průřez 0,5-1,5mm2 / délka 10mm, průměr špičky 1,9mm izolace PC s trychtýřem","100ks",5.9751123580910814,{"$f":"F522*(1-Elteq!$F$9)","v":5.9751123580910814},"8591735011741"]
["TECHNIK","KI 1,5-12",null,"Kolík izolovaný, průřez 0,5-1,5mm2 / délka 12mm, průměr špičky 1,9mm izolace PVC","100ks",5.2699748748380966,{"$f":"F523*(1-Elteq!$F$9)","v":5.2699748748380966},"8591735003531"]
["TECHNIK","KI 1,5-12/E",null,"Kolík izolovaný, průřez 0,5-1,5mm2 / délka 12mm, průměr špičky 1,9mm izolace PVC s trychtýřem","100ks",5.5297623686681439,{"$f":"F524*(1-Elteq!$F$9)","v":5.5297623686681439},"8591735027186"]
["TECHNIK","KI 1,5-12/PC",null,"Kolík izolovaný, průřez 0,5-1,5mm2 / délka 12mm, průměr špičky 1,9mm izolace PC s trychtýřem","100ks",6.0864498554468156,{"$f":"F525*(1-Elteq!$F$9)","v":6.0864498554468156},"8591735010485"]
["TECHNIK","KI 1,5-12/PK",null,"Kolík izolovaný, průřez 0,5-1,5mm2 / délka 12mm, průměr špičky 1,9mm izolace PC s Cu trychtýřem","100ks",11.356424730284912,{"$f":"F526*(1-Elteq!$F$9)","v":11.356424730284912},"8591735034047"]
["TECHNIK","KI 1,5-16",null,"Kolík izolovaný, průřez 0,5-1,5mm2 / délka 16mm, průměr špičky 1,9mm izolace PVC","100ks",6.9771498342926916,{"$f":"F527*(1-Elteq!$F$9)","v":6.9771498342926916},"8591735031954"]
["TECHNIK","KI 2,5- 8",null,"Kolík izolovaný, průřez 1,5-2,5mm2 / délka 8mm, průměr špičky 1,9mm izolace PVC","100ks",5.0472998801266282,{"$f":"F528*(1-Elteq!$F$9)","v":5.0472998801266282},"8591735003548"]
["TECHNIK","KI 2,5- 8/PC",null,"Kolík izolovaný, průřez 1,5-2,5mm2 / délka 8mm, průměr špičky 1,9mm izolace PC s trychtýřem","100ks",7.0142623334112697,{"$f":"F529*(1-Elteq!$F$9)","v":7.0142623334112697},"8591735011758"]
["TECHNIK","KI 2,5-10",null,"Kolík izolovaný, průřez 1,5-2,5mm2 / délka 10mm, průměr špičky 1,9mm izolace PVC","100ks",5.2699748748380966,{"$f":"F530*(1-Elteq!$F$9)","v":5.2699748748380966},"8591735003555"]
["TECHNIK","KI 2,5-10/E",null,"Kolík izolovaný, průřez 1,5-2,5mm2 / délka 10mm, průměr špičky 1,9mm izolace PVC s trychtýřem","100ks",5.7524373633796122,{"$f":"F531*(1-Elteq!$F$9)","v":5.7524373633796122},"8591735027193"]
["TECHNIK","KI 2,5-12",null,"Kolík izolovaný, průřez 1,5-2,5mm2 / délka 12mm, průměr špičky 1,9mm izolace PVC","100ks",5.6039873669053,{"$f":"F532*(1-Elteq!$F$9)","v":5.6039873669053},"8591735003562"]
["TECHNIK","KI 2,5-12/E",null,"Kolík izolovaný, průřez 1,5-2,5mm2 / délka 12mm, průměr špičky 1,9mm izolace PVC s trychtýřem","100ks",5.9379998589725034,{"$f":"F533*(1-Elteq!$F$9)","v":5.9379998589725034},"8591735027209"]
["TECHNIK","KI 2,5-12/PC",null,"Kolík izolovaný, průřez 1,5-2,5mm2 / délka 12mm, průměr špičky 1,9mm izolace PC s trychtýřem","100ks",7.0142623334112697,{"$f":"F534*(1-Elteq!$F$9)","v":7.0142623334112697},"8591735010492"]
["TECHNIK","KI 2,5-17",null,"Kolík izolovaný, průřez 1,5-2,5mm2 / délka 17mm, průměr špičky 1,9mm izolace PVC","100ks",7.1627123298855819,{"$f":"F535*(1-Elteq!$F$9)","v":7.1627123298855819},"8591735011727"]
["TECHNIK","KI 2,5-17/PC",null,"Kolík izolovaný, průřez 1,5-2,5mm2 / délka 17mm, průměr špičky 1,9mm izolace PC s trychtýřem","100ks",7.7193998166642546,{"$f":"F536*(1-Elteq!$F$9)","v":7.7193998166642546},"8591735011765"]
["TECHNIK","KI 6-10",null,"Kolík izolovaný, průřez 4,0-6,0mm2 / délka 10mm, průměr špičky 2,8mm izolace PVC s trychtýřem","100ks",8.7956622911030209,{"$f":"F537*(1-Elteq!$F$9)","v":8.7956622911030209},"8591735003579"]
["TECHNIK","KI 6-12",null,"Kolík izolovaný, průřez 4,0-6,0mm2 / délka 12mm, průměr špičky 2,8mm izolace PVC s trychtýřem","100ks",9.2781247796445356,{"$f":"F538*(1-Elteq!$F$9)","v":9.2781247796445356},"8591735003586"]
["TECHNIK","KI 6-14",null,"Kolík izolovaný, průřez 4,0-6,0mm2 / délka 14mm, průměr špičky 2,8mm izolace PVC","100ks",9.4636872752374277,{"$f":"F539*(1-Elteq!$F$9)","v":9.4636872752374277},"8591735003593"]
["TECHNIK","KI 6-14/E",null,"Kolík izolovaný, průřez 4,0-6,0mm2 / délka 14mm, průměr špičky 2,8mm izolace PVC s trychtýřem","100ks",9.7976997673046302,{"$f":"F540*(1-Elteq!$F$9)","v":9.7976997673046302},"8591735027216"]
["TECHNIK","KI 6-14/PC",null,"Kolík izolovaný, průřez 4,0-6,0mm2 / délka 14mm, průměr špičky 2,8mm izolace PC s trychtýřem","100ks",10.094599760253256,{"$f":"F541*(1-Elteq!$F$9)","v":10.094599760253256},"8591735010508"]
["TECHNIK","KI10-12",null,"Kolík izolovaný, průřez 10mm2, délka 12mm, izolace PA, barva černá","100ks",28.576624321305172,{"$f":"F542*(1-Elteq!$F$9)","v":28.576624321305172},"8591735003609"]
["TECHNIK","KI10-12.",null,"Kolík izolovaný, průřez 10mm2, délka 12mm, izolace PA, barva červená","100ks",27.092124356562046,{"$f":"F543*(1-Elteq!$F$9)","v":27.092124356562046},"8591735036829"]
["TECHNIK","KI16-14",null,"Kolík izolovaný, průřez 16mm2, délka 14mm, izolace PA, barva černá","100ks",32.287874233162988,{"$f":"F544*(1-Elteq!$F$9)","v":32.287874233162988},"8591735003616"]
["TECHNIK","KI16-14.",null,"Kolík izolovaný, průřez 16mm2, délka 14mm, izolace PA, barva modrá","100ks",30.803374268419862,{"$f":"F545*(1-Elteq!$F$9)","v":30.803374268419862},"8591735036836"]
["TECHNIK","KI25-16",null,"Kolík izolovaný, průřez 25mm2, délka 16mm, izolace PA, barva černá","100ks",54.184248713124092,{"$f":"F546*(1-Elteq!$F$9)","v":54.184248713124092},"8591735003623"]
["TECHNIK","KI25-16.",null,"Kolík izolovaný, průřez 25mm2, délka 16mm, izolace PA, barva žlutá","100ks",51.58637377482362,{"$f":"F547*(1-Elteq!$F$9)","v":51.58637377482362},"8591735036843"]
["TECHNIK","KI35-20",null,"Kolík izolovaný, průřez 35mm2, délka 20mm, izolace PA, barva černá","50ks",39.339249065692833,{"$f":"F548*(1-Elteq!$F$9)","v":39.339249065692833},"8591735003630"]
["TECHNIK","KI35-20.",null,"Kolík izolovaný, průřez 35mm2, délka 20mm, izolace PA, barva červená","50ks",37.48362410976393,{"$f":"F549*(1-Elteq!$F$9)","v":37.48362410976393},"8591735036850"]
["TECHNIK","KI50-26",null,"Kolík izolovaný, průřez 50mm2, délka 26mm, izolace PA, barva modrá","50ks",125.44024702079413,{"$f":"F550*(1-Elteq!$F$9)","v":125.44024702079413},"8591735003647"]
["TECHNIK","KI70-31",null,"Kolík izolovaný, průřez 70mm2, délka 31mm, izolace PA, barva žlutá","25ks",97.791435177453408,{"$f":"F551*(1-Elteq!$F$9)","v":97.791435177453408},"8591735003654"]
["TECHNIK","KI95-31",null,"Kolík izolovaný, průřez 95mm2, délka 31mm, izolace PA, barva červená","25ks",124.88355953401546,{"$f":"F552*(1-Elteq!$F$9)","v":124.88355953401546},"8591735003661"]
["TECHNIK","KIPL 0,5- 8",null,"Kolík plochý izolovaný, průřez 0,2-0,5mm2 / délka 8mm, izolace PVC","100ks",4.8988498836523151,{"$f":"F553*(1-Elteq!$F$9)","v":4.8988498836523151},"8591735031961"]
["TECHNIK","KIPL 1,5-12",null,"Kolík plochý izolovaný, průřez 0,5-1,5mm2 / délka 12mm, izolace PVC","100ks",4.7503998871780029,{"$f":"F554*(1-Elteq!$F$9)","v":4.7503998871780029},"8591735013059"]
["TECHNIK","KIPL 1,5-18",null,"Kolík plochý izolovaný, průřez 0,5-1,5mm2 / délka 18mm, izolace PVC","100ks",5.4555373704309877,{"$f":"F555*(1-Elteq!$F$9)","v":5.4555373704309877},"8591735015886"]
["TECHNIK","KIPL 2,5-12",null,"Kolík plochý izolovaný, průřez 1,5-2,5mm2 / délka 12mm, izolace PVC","100ks",5.4555373704309877,{"$f":"F556*(1-Elteq!$F$9)","v":5.4555373704309877},"8591735013042"]
["TECHNIK","KIPL 2,5-18",null,"Kolík plochý izolovaný, průřez 1,5-2,5mm2 / délka 18mm, izolace PVC","100ks",5.5668748677867219,{"$f":"F557*(1-Elteq!$F$9)","v":5.5668748677867219},"8591735015893"]
["TECHNIK","KIPL 6-12",null,"Kolík plochý izolovaný, průřez 4,0-6,0mm2 / délka 12mm, izolace PVC","100ks",8.4616497990358166,{"$f":"F558*(1-Elteq!$F$9)","v":8.4616497990358166},"8591735013066"]
["TECHNIK","KIPL 6-16",null,"Kolík plochý izolovaný, průřez 4,0-6,0mm2 / délka 16mm, izolace PVC","100ks",10.168824758490413,{"$f":"F559*(1-Elteq!$F$9)","v":10.168824758490413},"8591735015909"]
["TECHNIK","KIPPL 1,5/30",null,"Kolík plochý izolovaný, průřez 0,5-1,5mm2 / šířka 3,0mm, izolace PVC","100ks",5.7524373633796122,{"$f":"F560*(1-Elteq!$F$9)","v":5.7524373633796122},"8591735024970"]
["TECHNIK","KIPPL 1,5/46",null,"Kolík plochý izolovaný, průřez 0,5-1,5mm2 / šířka 4,6mm, izolace PVC","100ks",6.2720123510397068,{"$f":"F561*(1-Elteq!$F$9)","v":6.2720123510397068},"8591735028428"]
["TECHNIK","KIPPL 2,5/30",null,"Kolík plochý izolovaný, průřez 1,5-2,5mm2 / šířka 3,0mm, izolace PVC","100ks",6.0493373563282375,{"$f":"F562*(1-Elteq!$F$9)","v":6.0493373563282375},"8591735024987"]
["TECHNIK","KIPPL 2,5/46",null,"Kolík plochý izolovaný, průřez 1,5-2,5mm2 / šířka 4,6mm, izolace PVC","100ks",6.5689123439883321,{"$f":"F563*(1-Elteq!$F$9)","v":6.5689123439883321},"8591735028435"]
["TECHNIK","KIPPL 6/30",null,"Kolík plochý izolovaný, průřez 4,0-6,0mm2 / šířka 3,0mm, izolace PVC","100ks",7.8678498131385668,{"$f":"F564*(1-Elteq!$F$9)","v":7.8678498131385668},"8591735024994"]
["TECHNIK","KIPPL 6/46",null,"Kolík plochý izolovaný, průřez 4,0-6,0mm2 / šířka 4,6mm, izolace PVC","100ks",8.9441122875773331,{"$f":"F565*(1-Elteq!$F$9)","v":8.9441122875773331},"8591735028442"]
["TECHNIK","KN   0,5-10",null,"Kolík lisovací neizolovaný Cu cínovaný, průřez 0,2-0,5mm2 / délka 10mm","100ks",2.4123124427075795,{"$f":"F566*(1-Elteq!$F$9)","v":2.4123124427075795},"8591735003678"]
["TECHNIK","KN   1,5- 8",null,"Kolík lisovací neizolovaný Cu cínovaný, průřez 0,5-1,5mm2 / délka 8mm","100ks",4.1937124003993302,{"$f":"F567*(1-Elteq!$F$9)","v":4.1937124003993302},"8591735003937"]
["TECHNIK","KN   1,5-10",null,"Kolík lisovací neizolovaný Cu cínovaný, průřez 0,5-1,5mm2 / délka 10mm","100ks",4.5277248924665336,{"$f":"F568*(1-Elteq!$F$9)","v":4.5277248924665336},"8591735010515"]
["TECHNIK","KN   1,5-12",null,"Kolík lisovací neizolovaný Cu cínovaný, průřez 0,5-1,5mm2 / délka 12mm","100ks",4.7132873880594248,{"$f":"F569*(1-Elteq!$F$9)","v":4.7132873880594248},"8591735003685"]
["TECHNIK","KN   1,5-16",null,"Kolík lisovací neizolovaný Cu cínovaný, průřez 0,5-1,5mm2 / délka 16mm","100ks",6.420462347514019,{"$f":"F570*(1-Elteq!$F$9)","v":6.420462347514019},"8591735031978"]
["TECHNIK","KN   2,5- 8",null,"Kolík lisovací neizolovaný Cu cínovaný, průřez 1,5-2,5mm2 / délka 8mm","100ks",4.5277248924665336,{"$f":"F571*(1-Elteq!$F$9)","v":4.5277248924665336},"8591735010522"]
["TECHNIK","KN   2,5-10",null,"Kolík lisovací neizolovaný Cu cínovaný, průřez 1,5-2,5mm2 / délka 10mm","100ks",5.7524373633796122,{"$f":"F572*(1-Elteq!$F$9)","v":5.7524373633796122},"8591735010539"]
["TECHNIK","KN   2,5-12",null,"Kolík lisovací neizolovaný Cu cínovaný, průřez 1,5-2,5mm2 / délka 12mm","100ks",5.8637748607353473,{"$f":"F573*(1-Elteq!$F$9)","v":5.8637748607353473},"8591735003692"]
["TECHNIK","KN   2,5-16",null,"Kolík lisovací neizolovaný Cu cínovaný, průřez 1,5-2,5mm2 / délka 16mm","100ks",6.9029248360555355,{"$f":"F574*(1-Elteq!$F$9)","v":6.9029248360555355},"8591735031985"]
["TECHNIK","KN   6-10",null,"Kolík lisovací neizolovaný Cu cínovaný, průřez 4-6mm2 / délka 10mm","100ks",11.541987225877804,{"$f":"F575*(1-Elteq!$F$9)","v":11.541987225877804},"8591735028466"]
["TECHNIK","KN   6-12",null,"Kolík lisovací neizolovaný Cu cínovaný, průřez 4-6mm2 / délka 12mm","100ks",10.577062248794771,{"$f":"F576*(1-Elteq!$F$9)","v":10.577062248794771},"8591735028473"]
["TECHNIK","KN   6-14",null,"Kolík lisovací neizolovaný Cu cínovaný, průřez 4-6mm2 / délka 14mm","100ks",8.9069997884587551,{"$f":"F577*(1-Elteq!$F$9)","v":8.9069997884587551},"8591735003708"]
["TECHNIK","KN  10",null,"Kolík lisovací neizolovaný Cu cínovaný, průřez 10mm2 / délka 15mm","100ks",27.092124356562046,{"$f":"F578*(1-Elteq!$F$9)","v":27.092124356562046},"8591735003715"]
["TECHNIK","KN  16",null,"Kolík lisovací neizolovaný Cu cínovaný, průřez 16mm2 / délka 18mm","100ks",33.030124215534549,{"$f":"F579*(1-Elteq!$F$9)","v":33.030124215534549},"8591735003722"]
["TECHNIK","KN  25",null,"Kolík lisovací neizolovaný Cu cínovaný, průřez 25mm2 / délka 20mm","100ks",55.29762368668144,{"$f":"F580*(1-Elteq!$F$9)","v":55.29762368668144},"8591735003739"]
["TECHNIK","KN  35",null,"Kolík lisovací neizolovaný Cu cínovaný, průřez 35mm2 / délka 25mm","100ks",82.389748043243486,{"$f":"F581*(1-Elteq!$F$9)","v":82.389748043243486},"8591735003746"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"KN  50",null,"Kolík lisovací neizolovaný Cu cínovaný, průřez 50mm2 / délka 26mm","50ks",58.637748607353473,{"$f":"F582*(1-Elteq!$F$9)","v":58.637748607353473},"8591735003753"]
["TECHNIK","KN  70",null,"Kolík lisovací neizolovaný Cu cínovaný, průřez 70mm2 / délka 31mm","50ks",86.843247937472867,{"$f":"F583*(1-Elteq!$F$9)","v":86.843247937472867},"8591735003760"]
["TECHNIK","KN  95",null,"Kolík lisovací neizolovaný Cu cínovaný, průřez 95mm2 / délka 31mm","50ks",150.3056214302415,{"$f":"F584*(1-Elteq!$F$9)","v":150.3056214302415},"8591735003777"]
["TECHNIK","KNPL 0,5- 8",null,"Kolík lisovací neizolovaný plochý Cu cínovaný, průřez 0,2-0,5mm2 / délka 8mm / šíře 1,5mm","100ks",2.820549933011939,{"$f":"F585*(1-Elteq!$F$9)","v":2.820549933011939},"8591735052355"]
["TECHNIK","KNPL 1,5-10",null,"Kolík lisovací neizolovaný plochý Cu cínovaný, průřez 0,5-1,5mm2 / délka 10mm / šíře 2,3mm","100ks",5.1215248783637843,{"$f":"F586*(1-Elteq!$F$9)","v":5.1215248783637843},"8591735052362"]
["TECHNIK","KNPL 1,5-14",null,"Kolík lisovací neizolovaný plochý Cu cínovaný, průřez 0,5-1,5mm2 / délka 14mm / šíře 3mm","100ks",5.7153248642610341,{"$f":"F587*(1-Elteq!$F$9)","v":5.7153248642610341},"8591735052379"]
["TECHNIK","KNPL 1,5-18",null,"Kolík lisovací neizolovaný plochý Cu cínovaný, průřez 0,5-1,5mm2 / délka 18mm / šíře 2,2mm","100ks",5.9008873598539253,{"$f":"F588*(1-Elteq!$F$9)","v":5.9008873598539253},"8591735052386"]
["TECHNIK","KNPL 2,5-10",null,"Kolík lisovací neizolovaný plochý Cu cínovaný, průřez 1,5-2,5mm2 / délka 10mm / šíře 2,4mm","100ks",6.1235623545653937,{"$f":"F589*(1-Elteq!$F$9)","v":6.1235623545653937},"8591735052393"]
["TECHNIK","KNPL 2,5-14",null,"Kolík lisovací neizolovaný plochý Cu cínovaný, průřez 1,5-2,5mm2 / délka 14mm / šíře 2,4mm","100ks",6.7544748395812224,{"$f":"F590*(1-Elteq!$F$9)","v":6.7544748395812224},"8591735052409"]
["TECHNIK","KNPL 2,5-18",null,"Kolík lisovací neizolovaný plochý Cu cínovaný, průřez 1,5-2,5mm2 / délka 18mm / šíře 2,2mm","100ks",7.3482748254784731,{"$f":"F591*(1-Elteq!$F$9)","v":7.3482748254784731},"8591735052416"]
["TECHNIK","KNPL 6-10",null,"Kolík lisovací neizolovaný plochý Cu cínovaný, průřez 4,0-6,0mm2 / délka 10mm / šíře 2,8mm","100ks",10.836849742624819,{"$f":"F592*(1-Elteq!$F$9)","v":10.836849742624819},"8591735052423"]
["TECHNIK","KNPL 6-14",null,"Kolík lisovací neizolovaný plochý Cu cínovaný, průřez 4,0-6,0mm2 / délka 14mm / šíře 4,5mm","100ks",11.430649728522068,{"$f":"F593*(1-Elteq!$F$9)","v":11.430649728522068},"8591735052430"]
["TECHNIK","KNPL 6-18",null,"Kolík lisovací neizolovaný plochý Cu cínovaný, průřez 4,0-6,0mm2 / délka 18mm / šíře 4,5mm","100ks",13.880074670348227,{"$f":"F594*(1-Elteq!$F$9)","v":13.880074670348227},"8591735052447"]
["TECHNIK","KKC 1,5-4/PA",null,"Kolík kruhový celoizolovaný, průřez 0,5-1,5mm2 / průměr 4mm PA","100ks",8.3503123016800824,{"$f":"F595*(1-Elteq!$F$9)","v":8.3503123016800824},"8591735020309"]
["TECHNIK","KKC 1,5-4/PC",null,"Kolík kruhový celoizolovaný, průřez 0,5-1,5mm2 / průměr 4mm PC","100ks",9.2410122805259576,{"$f":"F596*(1-Elteq!$F$9)","v":9.2410122805259576},"8591735013295"]
["TECHNIK","KKC 2,5-4/PC",null,"Kolík kruhový celoizolovaný, průřez 1,5-2,5mm2 / průměr 4mm PC","100ks",9.7234747690674741,{"$f":"F597*(1-Elteq!$F$9)","v":9.7234747690674741},"8591735013301"]
["TECHNIK","KKP 1,5-4",null,"Kolík kruhový poloizolovaný, průřez 0,5-1,5mm2 / průměr 4mm PVC","100ks",5.0844123792452063,{"$f":"F598*(1-Elteq!$F$9)","v":5.0844123792452063},"8591735005382"]
["TECHNIK","KKP 1,5-4/PA",null,"Kolík kruhový poloizolovaný, průřez 0,5-1,5mm2 / průměr 4mm PA","100ks",9.4636872752374277,{"$f":"F599*(1-Elteq!$F$9)","v":9.4636872752374277},"8591735020316"]
["TECHNIK","KKP 1,5-4/PC",null,"Kolík kruhový poloizolovaný, průřez 0,5-1,5mm2 / průměr 4mm PC","100ks",9.6121372717117399,{"$f":"F600*(1-Elteq!$F$9)","v":9.6121372717117399},"8591735012526"]
["TECHNIK","KKP 2,5-4",null,"Kolík kruhový poloizolovaný, průřez 1,5-2,5mm2 / průměr 4mm PVC","100ks",5.9379998589725034,{"$f":"F601*(1-Elteq!$F$9)","v":5.9379998589725034},"8591735012489"]
["TECHNIK","KKP 2,5-4/PC",null,"Kolík kruhový poloizolovaný, průřez 1,5-2,5mm2 / průměr 4mm PC","100ks",9.2781247796445356,{"$f":"F602*(1-Elteq!$F$9)","v":9.2781247796445356},"8591735012533"]
["TECHNIK","KKP 2,5-5",null,"Kolík kruhový poloizolovaný, průřez 1,5-2,5mm2 / průměr 5mm PVC","100ks",5.9379998589725034,{"$f":"F603*(1-Elteq!$F$9)","v":5.9379998589725034},"8591735005405"]
["TECHNIK","KKP 2,5-5/PC",null,"Kolík kruhový poloizolovaný, průřez 1,5-2,5mm2 / průměr 5mm PC","100ks",9.2781247796445356,{"$f":"F604*(1-Elteq!$F$9)","v":9.2781247796445356},"8591735012540"]
["TECHNIK","KKP 6-5",null,"Kolík kruhový poloizolovaný, průřez 4-6mm2 / průměr 5mm PVC","100ks",8.5358747972729727,{"$f":"F605*(1-Elteq!$F$9)","v":8.5358747972729727},"8591735005412"]
["TECHNIK","KKP 6-5/PC",null,"Kolík kruhový poloizolovaný, průřez 4-6mm2 / průměr 5mm PC","100ks",12.321349707367945,{"$f":"F606*(1-Elteq!$F$9)","v":12.321349707367945},"8591735012557"]
["TECHNIK","KPC 1,5-68/PA",null,"Kolík plochý celoizolovaný, průřez 0,5-1,5mm2 / 6,3x0,8mm PA","100ks",10.948187239980554,{"$f":"F607*(1-Elteq!$F$9)","v":10.948187239980554},"8591735005429"]
["TECHNIK","KPC 2,5-68/PA",null,"Kolík plochý celoizolovaný, průřez 1,5-2,5mm2 / 6,3x0,8mm PA","100ks",11.133749735573444,{"$f":"F608*(1-Elteq!$F$9)","v":11.133749735573444},"8591735005436"]
["TECHNIK","KPC 6-68/PA",null,"Kolík plochý celoizolovaný, průřez 4-6mm2 / 6,3x0,8mm PA","100ks",11.39353722940349,{"$f":"F609*(1-Elteq!$F$9)","v":11.39353722940349},"8591735005443"]
["TECHNIK","KPP 1,5-25",null,"Kolík plochý poloizolovaný, průřez 0,5-1,5mm2 / 2,8x0,5mm PVC","100ks",5.3441998730752527,{"$f":"F610*(1-Elteq!$F$9)","v":5.3441998730752527},"8591735005450"]
["TECHNIK","KPP 1,5-25/PC",null,"Kolík plochý poloizolovaný, průřez 0,5-1,5mm2 / 2,8x0,5mm PC","100ks",8.869887289340177,{"$f":"F611*(1-Elteq!$F$9)","v":8.869887289340177},"8591735011475"]
["TECHNIK","KPP 1,5-28",null,"Kolík plochý poloizolovaný, průřez 0,5-1,5mm2 / 2,8x0,8mm PVC","100ks",5.3441998730752527,{"$f":"F612*(1-Elteq!$F$9)","v":5.3441998730752527},"8591735005467"]
["TECHNIK","KPP 1,5-28/PC",null,"Kolík plochý poloizolovaný, průřez 0,5-1,5mm2 / 2,8x0,8mm PC","100ks",8.869887289340177,{"$f":"F613*(1-Elteq!$F$9)","v":8.869887289340177},"8591735011482"]
["TECHNIK","KPP 1,5-45",null,"Kolík plochý poloizolovaný, průřez 0,5-1,5mm2 / 4,8x0,5mm PVC","100ks",5.7153248642610341,{"$f":"F614*(1-Elteq!$F$9)","v":5.7153248642610341},"8591735005474"]
["TECHNIK","KPP 1,5-45/PC",null,"Kolík plochý poloizolovaný, průřez 0,5-1,5mm2 / 4,8x0,5mm PC","100ks",10.168824758490413,{"$f":"F615*(1-Elteq!$F$9)","v":10.168824758490413},"8591735005481"]
["TECHNIK","KPP 1,5-48",null,"Kolík plochý poloizolovaný, průřez 0,5-1,5mm2 / 4,8x0,8mm PVC","100ks",5.7153248642610341,{"$f":"F616*(1-Elteq!$F$9)","v":5.7153248642610341},"8591735005498"]
["TECHNIK","KPP 1,5-48/PA",null,"Kolík plochý poloizolovaný, průřez 0,5-1,5mm2 / 4,8x0,8mm PA","100ks",10.577062248794771,{"$f":"F617*(1-Elteq!$F$9)","v":10.577062248794771},"8591735040888"]
["TECHNIK","KPP 1,5-48/PC",null,"Kolík plochý poloizolovaný, průřez 0,5-1,5mm2 / 4,8x0,8mm PC","100ks",10.168824758490413,{"$f":"F618*(1-Elteq!$F$9)","v":10.168824758490413},"8591735005504"]
["TECHNIK","KPP 1,5-68",null,"Kolík plochý poloizolovaný, průřez 0,5-1,5mm2 / 6,3x0,8mm PVC","100ks",5.9379998589725034,{"$f":"F619*(1-Elteq!$F$9)","v":5.9379998589725034},"8591735005511"]
["TECHNIK","KPP 1,5-68/PA",null,"Kolík plochý poloizolovaný, průřez 0,5-1,5mm2 / 6,3x0,8mm PA","100ks",7.3482748254784731,{"$f":"F620*(1-Elteq!$F$9)","v":7.3482748254784731},"8591735032098"]
["TECHNIK","KPP 1,5-68/PC",null,"Kolík plochý poloizolovaný, průřez 0,5-1,5mm2 / 6,3x0,8mm PC","100ks",7.8307373140199887,{"$f":"F621*(1-Elteq!$F$9)","v":7.8307373140199887},"8591735010980"]
["TECHNIK","KPP 2,5-45",null,"Kolík plochý poloizolovaný, průřez 1,5-2,5mm2 / 4,8x0,5mm PVC","100ks",5.7153248642610341,{"$f":"F622*(1-Elteq!$F$9)","v":5.7153248642610341},"8591735005528"]
["TECHNIK","KPP 2,5-45/PC",null,"Kolík plochý poloizolovaný, průřez 1,5-2,5mm2 / 4,8x0,5mm PC","100ks",9.6121372717117399,{"$f":"F623*(1-Elteq!$F$9)","v":9.6121372717117399},"8591735011499"]
["TECHNIK","KPP 2,5-48",null,"Kolík plochý poloizolovaný, průřez 1,5-2,5mm2 / 4,8x0,8mm PVC","100ks",5.7153248642610341,{"$f":"F624*(1-Elteq!$F$9)","v":5.7153248642610341},"8591735005535"]
["TECHNIK","KPP 2,5-48/PA",null,"Kolík plochý poloizolovaný, průřez 1,5-2,5mm2 / 4,8x0,8mm PA","100ks",10.243049756727569,{"$f":"F625*(1-Elteq!$F$9)","v":10.243049756727569},"8591735040895"]
["TECHNIK","KPP 2,5-48/PC",null,"Kolík plochý poloizolovaný, průřez 1,5-2,5mm2 / 4,8x0,8mm PC","100ks",9.6121372717117399,{"$f":"F626*(1-Elteq!$F$9)","v":9.6121372717117399},"8591735011505"]
["TECHNIK","KPP 2,5-68",null,"Kolík plochý poloizolovaný, průřez 1,5-2,5mm2 / 6,3x0,8mm PVC","100ks",5.9008873598539253,{"$f":"F627*(1-Elteq!$F$9)","v":5.9008873598539253},"8591735005542"]
["TECHNIK","KPP 2,5-68/PA",null,"Kolík plochý poloizolovaný, průřez 1,5-2,5mm2 / 6,3x0,8mm PA","100ks",7.311162326359895,{"$f":"F628*(1-Elteq!$F$9)","v":7.311162326359895},"8591735040833"]
["TECHNIK","KPP 2,5-68/PC",null,"Kolík plochý poloizolovaný, průřez 1,5-2,5mm2 / 6,3x0,8mm PC","100ks",9.7234747690674741,{"$f":"F629*(1-Elteq!$F$9)","v":9.7234747690674741},"8591735010997"]
["TECHNIK","KPP 6-68",null,"Kolík plochý poloizolovaný, průřez 4-6mm2 / 6,3x0,8mm PVC","100ks",7.6080623193085195,{"$f":"F630*(1-Elteq!$F$9)","v":7.6080623193085195},"8591735005559"]
["TECHNIK","KPP 6-68/PA",null,"Kolík plochý poloizolovaný, průřez 4-6mm2 / 6,3x0,8mm PA","100ks",9.6121372717117399,{"$f":"F631*(1-Elteq!$F$9)","v":9.6121372717117399},"8591735040901"]
["TECHNIK","KPP 6-68/PC",null,"Kolík plochý poloizolovaný, průřez 4-6mm2 / 6,3x0,8mm PC","100ks",10.317274754964725,{"$f":"F632*(1-Elteq!$F$9)","v":10.317274754964725},"8591735011062"]
["TECHNIK","OKC 1,5-4",null,"Objímka kruhová celoizolovaná, průřez 0,5-1,5mm2 / průměr 4mm, PVC","100ks",5.9379998589725034,{"$f":"F633*(1-Elteq!$F$9)","v":5.9379998589725034},"8591735005566"]
["TECHNIK","OKC 1,5-4/PA",null,"Objímka kruhová celoizolovaná, průřez 0,5-1,5mm2 / průměr 4mm, PA","100ks",12.284237208249367,{"$f":"F634*(1-Elteq!$F$9)","v":12.284237208249367},"8591735025298"]
["TECHNIK","OKC 1,5-4/PC",null,"Objímka kruhová celoizolovaná, průřez 0,5-1,5mm2 / průměr 4mm, PC","100ks",12.469799703842257,{"$f":"F635*(1-Elteq!$F$9)","v":12.469799703842257},"8591735012564"]
["TECHNIK","OKC 2,5-4",null,"Objímka kruhová celoizolovaná, průřez 1,5-2,5mm2 / průměr 4mm, PVC","100ks",6.4946873457511751,{"$f":"F636*(1-Elteq!$F$9)","v":6.4946873457511751},"8591735012496"]
["TECHNIK","OKC 2,5-4/PA",null,"Objímka kruhová celoizolovaná, průřez 1,5-2,5mm2 / průměr 4mm, PA","100ks",11.690437222352116,{"$f":"F637*(1-Elteq!$F$9)","v":11.690437222352116},"8591735050535"]
["TECHNIK","OKC 2,5-4/PC",null,"Objímka kruhová celoizolovaná, průřez 1,5-2,5mm2 / průměr 4mm, PC","100ks",11.690437222352116,{"$f":"F638*(1-Elteq!$F$9)","v":11.690437222352116},"8591735012571"]
["TECHNIK","OKC 2,5-5",null,"Objímka kruhová celoizolovaná, průřez 1,5-2,5mm2 / průměr 5mm, PVC","100ks",6.4946873457511751,{"$f":"F639*(1-Elteq!$F$9)","v":6.4946873457511751},"8591735005580"]
["TECHNIK","OKC 2,5-5/PC",null,"Objímka kruhová celoizolovaná, průřez 1,5-2,5mm2 / průměr 5mm, PC","100ks",13.546062178281023,{"$f":"F640*(1-Elteq!$F$9)","v":13.546062178281023},"8591735012588"]
["TECHNIK","OKC 6-5",null,"Objímka kruhová celoizolovaná, průřez 4-6mm2 / průměr 5mm, PVC","100ks",10.577062248794771,{"$f":"F641*(1-Elteq!$F$9)","v":10.577062248794771},"8591735005597"]
["TECHNIK","OKC 6-5/PC",null,"Objímka kruhová celoizolovaná, průřez 4-6mm2 / průměr 5mm, PC","100ks",14.659437151838368,{"$f":"F642*(1-Elteq!$F$9)","v":14.659437151838368},"8591735012595"]
["TECHNIK","OKP 1,5-4",null,"Objímka kruhová poloizolovaná, průřez 0,5-1,5mm2 / průměr 4mm, PVC","100ks",9.2410122805259576,{"$f":"F643*(1-Elteq!$F$9)","v":9.2410122805259576},"8591735035013"]
["TECHNIK","OKP 1,5-4/PA",null,"Objímka kruhová poloizolovaná, průřez 0,5-1,5mm2 / průměr 4mm, PA","100ks",10.205937257608991,{"$f":"F644*(1-Elteq!$F$9)","v":10.205937257608991},"8591735035204"]
["TECHNIK","OKP 2,5-4",null,"Objímka kruhová poloizolovaná, průřez 1,5-2,5mm2 / průměr 4mm, PVC","100ks",9.4636872752374277,{"$f":"F645*(1-Elteq!$F$9)","v":9.4636872752374277},"8591735035020"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"OKP 2,5-4/PA",null,"Objímka kruhová poloizolovaná, průřez 1,5-2,5mm2 / průměr 4mm, PA","100ks",10.317274754964725,{"$f":"F646*(1-Elteq!$F$9)","v":10.317274754964725},"8591735035211"]
["TECHNIK","OKP 2,5-5",null,"Objímka kruhová poloizolovaná, průřez 1,5-2,5mm2 / průměr 5mm, PVC","100ks",9.9461497637789424,{"$f":"F647*(1-Elteq!$F$9)","v":9.9461497637789424},"8591735035037"]
["TECHNIK","OKP 2,5-5/PA",null,"Objímka kruhová poloizolovaná, průřez 1,5-2,5mm2 / průměr 5mm, PA","100ks",10.688399746150505,{"$f":"F648*(1-Elteq!$F$9)","v":10.688399746150505},"8591735035228"]
["TECHNIK","OKP 6-5",null,"Objímka kruhová poloizolovaná, průřez 4-6mm2 / průměr 5mm, PVC","100ks",18.890262051356277,{"$f":"F649*(1-Elteq!$F$9)","v":18.890262051356277},"8591735035044"]
["TECHNIK","OKP 6-5/PA",null,"Objímka kruhová poloizolovaná, průřez 4-6mm2 / průměr 5mm, PA","100ks",20.374762016099403,{"$f":"F650*(1-Elteq!$F$9)","v":20.374762016099403},"8591735035235"]
["TECHNIK","OPC 0,5-25/PA",null,"Objímka plochá celoizolovaná, průřez 0,2-0,5mm2 / 2,8x0,5mm PA fialová","100ks",11.282199732047756,{"$f":"F651*(1-Elteq!$F$9)","v":11.282199732047756},"8591735034207"]
["TECHNIK","OPC 0,5-28/PA",null,"Objímka plochá celoizolovaná, průřez 0,2-0,5mm2 / 2,8x0,8mm PA fialová","100ks",11.282199732047756,{"$f":"F652*(1-Elteq!$F$9)","v":11.282199732047756},"8591735034214"]
["TECHNIK","OPC 0,5-45/PA",null,"Objímka plochá celoizolovaná, průřez 0,2-0,5mm2 / 4,8x0,5mm PA fialová","100ks",12.284237208249367,{"$f":"F653*(1-Elteq!$F$9)","v":12.284237208249367},"8591735034221"]
["TECHNIK","OPC 0,5-48/PA",null,"Objímka plochá celoizolovaná, průřez 0,2-0,5mm2 / 4,8x0,8mm PA fialová","100ks",12.284237208249367,{"$f":"F654*(1-Elteq!$F$9)","v":12.284237208249367},"8591735034238"]
["TECHNIK","OPC 1,5-25",null,"Objímka plochá celoizolovaná, průřez 0,5-1,5mm2 / 2,8x0,5mm PVC","100ks",7.3482748254784731,{"$f":"F655*(1-Elteq!$F$9)","v":7.3482748254784731},"8591735011079"]
["TECHNIK","OPC 1,5-25/PA",null,"Objímka plochá celoizolovaná, průřez 0,5-1,5mm2 / 2,8x0,5mm PA","100ks",11.838887218826429,{"$f":"F656*(1-Elteq!$F$9)","v":11.838887218826429},"8591735055974"]
["TECHNIK","OPC 1,5-25/PC",null,"Objímka plochá celoizolovaná, průřez 0,5-1,5mm2 / 2,8x0,5mm PC","100ks",10.094599760253256,{"$f":"F657*(1-Elteq!$F$9)","v":10.094599760253256},"8591735005603"]
["TECHNIK","OPC 1,5-28",null,"Objímka plochá celoizolovaná, průřez 0,5-1,5mm2 / 2,8x0,8mm PVC","100ks",7.3482748254784731,{"$f":"F658*(1-Elteq!$F$9)","v":7.3482748254784731},"8591735011055"]
["TECHNIK","OPC 1,5-28/PA",null,"Objímka plochá celoizolovaná, průřez 0,5-1,5mm2 / 2,8x0,8mm PA","100ks",12.432687204723679,{"$f":"F659*(1-Elteq!$F$9)","v":12.432687204723679},"8591735056414"]
["TECHNIK","OPC 1,5-28/PC",null,"Objímka plochá celoizolovaná, průřez 0,5-1,5mm2 / 2,8x0,8mm PC","100ks",10.094599760253256,{"$f":"F660*(1-Elteq!$F$9)","v":10.094599760253256},"8591735005627"]
["TECHNIK","OPC 1,5-45",null,"Objímka plochá celoizolovaná, průřez 0,5-1,5mm2 / 4,8x0,5mm PVC","100ks",5.9008873598539253,{"$f":"F661*(1-Elteq!$F$9)","v":5.9008873598539253},"8591735005641"]
["TECHNIK","OPC 1,5-45/PC",null,"Objímka plochá celoizolovaná, průřez 0,5-1,5mm2 / 4,8x0,5mm PC","100ks",10.502837250557615,{"$f":"F662*(1-Elteq!$F$9)","v":10.502837250557615},"8591735005658"]
["TECHNIK","OPC 1,5-48",null,"Objímka plochá celoizolovaná, průřez 0,5-1,5mm2 / 4,8x0,8mm PVC","100ks",5.9008873598539253,{"$f":"F663*(1-Elteq!$F$9)","v":5.9008873598539253},"8591735005665"]
["TECHNIK","OPC 1,5-48/PC",null,"Objímka plochá celoizolovaná, průřez 0,5-1,5mm2 / 4,8x0,8mm PC","100ks",10.502837250557615,{"$f":"F664*(1-Elteq!$F$9)","v":10.502837250557615},"8591735006068"]
["TECHNIK","OPC 1,5-68",null,"Objímka plochá celoizolovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm PVC","100ks",6.6802498413440663,{"$f":"F665*(1-Elteq!$F$9)","v":6.6802498413440663},"8591735005689"]
["TECHNIK","OPC 1,5-68 BP/PA",null,"Objímka plochá celoizolovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm PA s bočním připojením","100ks",10.873962241743397,{"$f":"F666*(1-Elteq!$F$9)","v":10.873962241743397},"8591735033859"]
["TECHNIK","OPC 1,5-68 BP/PC",null,"Objímka plochá celoizolovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm PC s bočním připojením","100ks",8.7214372928658648,{"$f":"F667*(1-Elteq!$F$9)","v":8.7214372928658648},"8591735021702"]
["TECHNIK","OPC 1,5-68/OBD",null,"Objímka plochá celoizolovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm PVC","100ks",6.9029248360555355,{"$f":"F668*(1-Elteq!$F$9)","v":6.9029248360555355},"8591735012502"]
["TECHNIK","OPC 1,5-68/PA",null,"Objímka plochá celoizolovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm PA","100ks",7.7193998166642546,{"$f":"F669*(1-Elteq!$F$9)","v":7.7193998166642546},"8591735017989"]
["TECHNIK","OPC 1,5-68/PC",null,"Objímka plochá celoizolovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm PC","100ks",7.1627123298855819,{"$f":"F670*(1-Elteq!$F$9)","v":7.1627123298855819},"8591735005696"]
["TECHNIK","OPC 2,5-25/PA",null,"Objímka plochá celoizolovaná, průřez 1,5-2,5mm2 / 2,8x0,5mm PA","100ks",10.948187239980554,{"$f":"F671*(1-Elteq!$F$9)","v":10.948187239980554},"8591735034276"]
["TECHNIK","OPC 2,5-28/PA",null,"Objímka plochá celoizolovaná, průřez 1,5-2,5mm2 / 2,8x0,8mm PA","100ks",10.948187239980554,{"$f":"F672*(1-Elteq!$F$9)","v":10.948187239980554},"8591735034283"]
["TECHNIK","OPC 2,5-45",null,"Objímka plochá celoizolovaná, průřez 1,5-2,5mm2 / 4,8x0,5mm PVC","100ks",5.9751123580910814,{"$f":"F673*(1-Elteq!$F$9)","v":5.9751123580910814},"8591735005719"]
["TECHNIK","OPC 2,5-45/PC",null,"Objímka plochá celoizolovaná, průřez 1,5-2,5mm2 / 4,8x0,5mm PC","100ks",10.911074740861975,{"$f":"F674*(1-Elteq!$F$9)","v":10.911074740861975},"8591735005238"]
["TECHNIK","OPC 2,5-48",null,"Objímka plochá celoizolovaná, průřez 1,5-2,5mm2 / 4,8x0,8mm PVC","100ks",5.9751123580910814,{"$f":"F675*(1-Elteq!$F$9)","v":5.9751123580910814},"8591735005726"]
["TECHNIK","OPC 2,5-48/PC",null,"Objímka plochá celoizolovaná, průřez 1,5-2,5mm2 / 4,8x0,8mm PC","100ks",10.911074740861975,{"$f":"F676*(1-Elteq!$F$9)","v":10.911074740861975},"8591735005115"]
["TECHNIK","OPC 2,5-68",null,"Objímka plochá celoizolovaná, průřez 1,5-2,5mm2 / 6,3x0,8mm PVC","100ks",7.0142623334112697,{"$f":"F677*(1-Elteq!$F$9)","v":7.0142623334112697},"8591735005733"]
["TECHNIK","OPC 2,5-68 BP/PA",null,"Objímka plochá celoizolovaná, průřez 1,5-2,5mm2 / 6,3x0,8mm PA s bočním připojením","100ks",11.801774719707851,{"$f":"F678*(1-Elteq!$F$9)","v":11.801774719707851},"8591735033866"]
["TECHNIK","OPC 2,5-68 BP/PC",null,"Objímka plochá celoizolovaná, průřez 1,5-2,5mm2 / 6,3x0,8mm PC s bočním připojením","100ks",9.7605872681860522,{"$f":"F679*(1-Elteq!$F$9)","v":9.7605872681860522},"8591735021696"]
["TECHNIK","OPC 2,5-68/OBD",null,"Objímka plochá celoizolovaná, průřez 1,5-2,5mm2 / 6,3x0,8mm PVC","100ks",7.0884873316484258,{"$f":"F680*(1-Elteq!$F$9)","v":7.0884873316484258},"8591735012519"]
["TECHNIK","OPC 2,5-68/PA",null,"Objímka plochá celoizolovaná, průřez 1,5-2,5mm2 / 6,3x0,8mm PA","100ks",12.061562213537897,{"$f":"F681*(1-Elteq!$F$9)","v":12.061562213537897},"8591735025274"]
["TECHNIK","OPC 2,5-68/PC",null,"Objímka plochá celoizolovaná, průřez 1,5-2,5mm2 / 6,3x0,8mm PC","100ks",10.985299739099132,{"$f":"F682*(1-Elteq!$F$9)","v":10.985299739099132},"8591735005740"]
["TECHNIK","OPC 6-68",null,"Objímka plochá celoizolovaná, průřez 4-6mm2 / 6,3x0,8mm PVC","100ks",10.688399746150505,{"$f":"F683*(1-Elteq!$F$9)","v":10.688399746150505},"8591735005764"]
["TECHNIK","OPC 6-68 BP/PA",null,"Objímka plochá celoizolovaná, průřez 4-6mm2 / 6,3x0,8mm PA s bočním připojením","100ks",13.174937187095242,{"$f":"F684*(1-Elteq!$F$9)","v":13.174937187095242},"8591735033873"]
["TECHNIK","OPC 6-68/PA",null,"Objímka plochá celoizolovaná, průřez 4-6mm2 / 6,3x0,8mm PA","100ks",13.954299668585383,{"$f":"F685*(1-Elteq!$F$9)","v":13.954299668585383},"8591735025250"]
["TECHNIK","OPC 6-68/PC",null,"Objímka plochá celoizolovaná, průřez 4-6mm2 / 6,3x0,8mm PC","100ks",14.548099654482634,{"$f":"F686*(1-Elteq!$F$9)","v":14.548099654482634},"8591735005771"]
["TECHNIK","OPC 6-91",null,"Objímka plochá celoizolovaná, průřez 4-6mm2 / 9,5x1,2mm PVC","100ks",12.80381219590946,{"$f":"F687*(1-Elteq!$F$9)","v":12.80381219590946},"8591735010591"]
["TECHNIK","OPC 6-91/PC",null,"Objímka plochá celoizolovaná, průřez 4-6mm2 / 9,5x1,2mm PC","100ks",16.181049615700072,{"$f":"F688*(1-Elteq!$F$9)","v":16.181049615700072},"8591735012601"]
["TECHNIK","OPO 1,5",null,"Objímka plochá odbočná poloizolovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm PVC","100ks",7.3482748254784731,{"$f":"F689*(1-Elteq!$F$9)","v":7.3482748254784731},"8591735005788"]
["TECHNIK","OPO 1,5/PA",null,"Objímka plochá odbočná poloizolovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm PA","100ks",10.799737243506241,{"$f":"F690*(1-Elteq!$F$9)","v":10.799737243506241},"8591735040826"]
["TECHNIK","OPO 1,5/PC",null,"Objímka plochá odbočná poloizolovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm PC","100ks",10.799737243506241,{"$f":"F691*(1-Elteq!$F$9)","v":10.799737243506241},"8591735005795"]
["TECHNIK","OPO 2,5",null,"Objímka plochá odbočná poloizolovaná, průřez 1,5-2,5mm2 / 6,3x0,8mm PVC","100ks",7.3482748254784731,{"$f":"F692*(1-Elteq!$F$9)","v":7.3482748254784731},"8591735005801"]
["TECHNIK","OPO 2,5/PA",null,"Objímka plochá odbočná poloizolovaná, průřez 1,5-2,5mm2 / 6,3x0,8mm PA","100ks",10.985299739099132,{"$f":"F693*(1-Elteq!$F$9)","v":10.985299739099132},"8591735040840"]
["TECHNIK","OPO 2,5/PC",null,"Objímka plochá odbočná poloizolovaná, průřez 1,5-2,5mm2 / 6,3x0,8mm PC","100ks",10.985299739099132,{"$f":"F694*(1-Elteq!$F$9)","v":10.985299739099132},"8591735011512"]
["TECHNIK","OPO 6",null,"Objímka plochá odbočná poloizolovaná, průřez 4-6mm2 / 6,3x0,8mm PVC","100ks",8.7585497919844428,{"$f":"F695*(1-Elteq!$F$9)","v":8.7585497919844428},"8591735005818"]
["TECHNIK","OPO 6/PC",null,"Objímka plochá odbočná poloizolovaná, průřez 4-6mm2 / 6,3x0,8mm PC","100ks",13.954299668585383,{"$f":"F696*(1-Elteq!$F$9)","v":13.954299668585383},"8591735011529"]
["TECHNIK","OPOC 1,5",null,"Objímka plochá odbočná celoizolovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm PA","100ks",12.395574705605101,{"$f":"F697*(1-Elteq!$F$9)","v":12.395574705605101},"8591735035242"]
["TECHNIK","OPOC 2,5",null,"Objímka plochá odbočná celoizolovaná, průřez 1,5-2,5mm2 / 6,3x0,8mm PA","100ks",13.02648719062093,{"$f":"F698*(1-Elteq!$F$9)","v":13.02648719062093},"8591735035259"]
["TECHNIK","OPP 0,5-25",null,"Objímka plochá poloizolovaná, průřez 0,1-0,5mm2 / 2,8x0,5mm PVC","100ks",5.0101873810080493,{"$f":"F699*(1-Elteq!$F$9)","v":5.0101873810080493},"8591735011802"]
["TECHNIK","OPP 0,5-28",null,"Objímka plochá poloizolovaná, průřez 0,1-0,5mm2 / 2,8x0,8mm PVC","100ks",3.6741374127392366,{"$f":"F700*(1-Elteq!$F$9)","v":3.6741374127392366},"8591735011819"]
["TECHNIK","OPP 1,5-25",null,"Objímka plochá poloizolovaná, průřez 0,5-1,5mm2 / 2,8x0,5mm PVC","100ks",4.5277248924665336,{"$f":"F701*(1-Elteq!$F$9)","v":4.5277248924665336},"8591735005825"]
["TECHNIK","OPP 1,5-25/PC",null,"Objímka plochá poloizolovaná, průřez 0,5-1,5mm2 / 2,8x0,5mm PC","100ks",7.4967248219527853,{"$f":"F702*(1-Elteq!$F$9)","v":7.4967248219527853},"8591735009410"]
["TECHNIK","OPP 1,5-28",null,"Objímka plochá poloizolovaná, průřez 0,5-1,5mm2 / 2,8x0,8mm PVC","100ks",4.5277248924665336,{"$f":"F703*(1-Elteq!$F$9)","v":4.5277248924665336},"8591735005832"]
["TECHNIK","OPP 1,5-28/PC",null,"Objímka plochá poloizolovaná, průřez 0,5-1,5mm2 / 2,8x0,8mm PC","100ks",7.4967248219527853,{"$f":"F704*(1-Elteq!$F$9)","v":7.4967248219527853},"8591735009809"]
["TECHNIK","OPP 1,5-45",null,"Objímka plochá poloizolovaná, průřez 0,5-1,5mm2 / 4,8x0,5mm PVC","100ks",4.6390623898222678,{"$f":"F705*(1-Elteq!$F$9)","v":4.6390623898222678},"8591735005849"]
["TECHNIK","OPP 1,5-45/PC",null,"Objímka plochá poloizolovaná, průřez 0,5-1,5mm2 / 4,8x0,5mm PC","100ks",7.7936248149014107,{"$f":"F706*(1-Elteq!$F$9)","v":7.7936248149014107},"8591735009403"]
["TECHNIK","OPP 1,5-48",null,"Objímka plochá poloizolovaná, průřez 0,5-1,5mm2 / 4,8x0,8mm PVC","100ks",4.6390623898222678,{"$f":"F707*(1-Elteq!$F$9)","v":4.6390623898222678},"8591735005856"]
["TECHNIK","OPP 1,5-48 role",null,"Objímka plochá poloizolovaná, průřez 0,5-1,5mm2 / 4,8x0,8mm PVC (cívka)","1000ks",70.216848332349855,{"$f":"F708*(1-Elteq!$F$9)","v":70.216848332349855},"8591735040734"]
["TECHNIK","OPP 1,5-48/PA",null,"Objímka plochá poloizolovaná, průřez 0,5-1,5mm2 / 4,8x0,8mm PA","100ks",7.7936248149014107,{"$f":"F709*(1-Elteq!$F$9)","v":7.7936248149014107},"8591735040857"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"OPP 1,5-48/PA role",null,"Objímka plochá poloizolovaná, průřez 0,5-1,5mm2 / 4,8x0,8mm PA (cívka)","1000ks",102.02226007697132,{"$f":"F710*(1-Elteq!$F$9)","v":102.02226007697132},"8591735040727"]
["TECHNIK","OPP 1,5-48/PC",null,"Objímka plochá poloizolovaná, průřez 0,5-1,5mm2 / 4,8x0,8mm PC","100ks",7.7936248149014107,{"$f":"F711*(1-Elteq!$F$9)","v":7.7936248149014107},"8591735009397"]
["TECHNIK","OPP 1,5-68",null,"Objímka plochá poloizolovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm PVC","100ks",5.1586373774823624,{"$f":"F712*(1-Elteq!$F$9)","v":5.1586373774823624},"8591735005863"]
["TECHNIK","OPP 1,5-68/PA",null,"Objímka plochá poloizolovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm PA","100ks",7.6822873175456765,{"$f":"F713*(1-Elteq!$F$9)","v":7.6822873175456765},"8591735032104"]
["TECHNIK","OPP 1,5-68/PC",null,"Objímka plochá poloizolovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm PC","100ks",8.053412308731458,{"$f":"F714*(1-Elteq!$F$9)","v":8.053412308731458},"8591735005870"]
["TECHNIK","OPP 2,5-25",null,"Objímka plochá poloizolovaná, průřez 1,5-2,5mm2 / 2,8x0,5mm PVC","100ks",5.1215248783637843,{"$f":"F715*(1-Elteq!$F$9)","v":5.1215248783637843},"8591735005887"]
["TECHNIK","OPP 2,5-25/PA",null,"Objímka plochá poloizolovaná, průřez 1,5-2,5mm2 / 2,8x0,5mm PA","100ks",7.6080623193085195,{"$f":"F716*(1-Elteq!$F$9)","v":7.6080623193085195},"8591735032111"]
["TECHNIK","OPP 2,5-25/PC",null,"Objímka plochá poloizolovaná, průřez 1,5-2,5mm2  / 2,8x0,5mm PC","100ks",7.6080623193085195,{"$f":"F717*(1-Elteq!$F$9)","v":7.6080623193085195},"8591735011536"]
["TECHNIK","OPP 2,5-28",null,"Objímka plochá poloizolovaná, průřez 1,5-2,5mm2 / 2,8x0,8mm PVC","100ks",5.1215248783637843,{"$f":"F718*(1-Elteq!$F$9)","v":5.1215248783637843},"8591735005894"]
["TECHNIK","OPP 2,5-28/PC",null,"Objímka plochá poloizolovaná, průřez 1,5-2,5mm2 / 2,8x0,8mm PC","100ks",7.6080623193085195,{"$f":"F719*(1-Elteq!$F$9)","v":7.6080623193085195},"8591735005061"]
["TECHNIK","OPP 2,5-45",null,"Objímka plochá poloizolovaná, průřez 1,5-2,5mm2 / 4,8x0,5mm PVC","100ks",5.4926498695495658,{"$f":"F720*(1-Elteq!$F$9)","v":5.4926498695495658},"8591735005900"]
["TECHNIK","OPP 2,5-45/PC",null,"Objímka plochá poloizolovaná, průřez 1,5-2,5mm2 / 4,8x0,5mm PC","100ks",6.4946873457511751,{"$f":"F721*(1-Elteq!$F$9)","v":6.4946873457511751},"8591735007331"]
["TECHNIK","OPP 2,5-48",null,"Objímka plochá poloizolovaná, průřez 1,5-2,5mm2 / 4,8x0,8mm PVC","100ks",5.4926498695495658,{"$f":"F722*(1-Elteq!$F$9)","v":5.4926498695495658},"8591735005917"]
["TECHNIK","OPP 2,5-48/PA",null,"Objímka plochá poloizolovaná, průřez 1,5-2,5mm2 / 4,8x0,8mm PA","100ks",7.6080623193085195,{"$f":"F723*(1-Elteq!$F$9)","v":7.6080623193085195},"8591735040864"]
["TECHNIK","OPP 2,5-48/PC",null,"Objímka plochá poloizolovaná, průřez 1,5-2,5mm2 / 4,8x0,8mm PC","100ks",6.4946873457511751,{"$f":"F724*(1-Elteq!$F$9)","v":6.4946873457511751},"8591735005610"]
["TECHNIK","OPP 2,5-68",null,"Objímka plochá poloizolovaná, průřez 1,5-2,5mm2 / 6,3x0,8mm PVC","100ks",4.861737384533737,{"$f":"F725*(1-Elteq!$F$9)","v":4.861737384533737},"8591735005924"]
["TECHNIK","OPP 2,5-68/PA",null,"Objímka plochá poloizolovaná, průřez 1,5-2,5mm2 / 6,3x0,8mm PA","100ks",9.1667872822888015,{"$f":"F726*(1-Elteq!$F$9)","v":9.1667872822888015},"8591735032128"]
["TECHNIK","OPP 2,5-68/PC",null,"Objímka plochá poloizolovaná, průřez 1,5-2,5mm2 / 6,3x0,8mm PC","100ks",9.4636872752374277,{"$f":"F727*(1-Elteq!$F$9)","v":9.4636872752374277},"8591735005931"]
["TECHNIK","OPP 2,5-91",null,"Objímka plochá poloizolovaná, průřez 1,5-2,5mm2 / 9,5x1,2mm PVC","100ks",10.725512245269083,{"$f":"F728*(1-Elteq!$F$9)","v":10.725512245269083},"8591735034245"]
["TECHNIK","OPP 6-25",null,"Objímka plochá poloizolovaná, průřez 4-6mm2 / 2,8x0,5mm PVC","100ks",10.020374762016099,{"$f":"F729*(1-Elteq!$F$9)","v":10.020374762016099},"8591735034252"]
["TECHNIK","OPP 6-28",null,"Objímka plochá poloizolovaná, průřez 4-6mm2 / 2,8x0,8mm PVC","100ks",10.020374762016099,{"$f":"F730*(1-Elteq!$F$9)","v":10.020374762016099},"8591735034269"]
["TECHNIK","OPP 6-45",null,"Objímka plochá poloizolovaná, průřez 4-6mm2 / 4,8x0,5mm PVC","100ks",8.3874248007986605,{"$f":"F731*(1-Elteq!$F$9)","v":8.3874248007986605},"8591735001544"]
["TECHNIK","OPP 6-45/PC",null,"Objímka plochá poloizolovaná, průřez 4-6mm2 / 4,8x0,5mm PC","100ks",10.539949749676193,{"$f":"F732*(1-Elteq!$F$9)","v":10.539949749676193},"8591735011543"]
["TECHNIK","OPP 6-48",null,"Objímka plochá poloizolovaná, průřez 4-6mm2 / 4,8x0,8mm PVC","100ks",8.3874248007986605,{"$f":"F733*(1-Elteq!$F$9)","v":8.3874248007986605},"8591735011468"]
["TECHNIK","OPP 6-48/PA",null,"Objímka plochá poloizolovaná, průřez 4-6mm2 / 4,8x0,8mm PA","100ks",11.059524737336288,{"$f":"F734*(1-Elteq!$F$9)","v":11.059524737336288},"8591735040871"]
["TECHNIK","OPP 6-48/PC",null,"Objímka plochá poloizolovaná, průřez 4-6mm2 / 4,8x0,8mm PC","100ks",10.539949749676193,{"$f":"F735*(1-Elteq!$F$9)","v":10.539949749676193},"8591735011550"]
["TECHNIK","OPP 6-68",null,"Objímka plochá poloizolovaná, průřez 4-6mm2 / 6,3x0,8mm PVC","100ks",8.1647498060871921,{"$f":"F736*(1-Elteq!$F$9)","v":8.1647498060871921},"8591735005948"]
["TECHNIK","OPP 6-68/PA",null,"Objímka plochá poloizolovaná, průřez 4-6mm2 / 6,3x0,8mm PA","100ks",11.096637236454866,{"$f":"F737*(1-Elteq!$F$9)","v":11.096637236454866},"8591735040819"]
["TECHNIK","OPP 6-68/PC",null,"Objímka plochá poloizolovaná, průřez 4-6mm2 / 6,3x0,8mm PC","100ks",11.356424730284912,{"$f":"F738*(1-Elteq!$F$9)","v":11.356424730284912},"8591735005955"]
["TECHNIK","OPP 6-91",null,"Objímka plochá poloizolovaná, průřez 4-6mm2 / 9,5x1,2mm PVC","100ks",10.391499753201881,{"$f":"F739*(1-Elteq!$F$9)","v":10.391499753201881},"8591735005962"]
["TECHNIK","OPP 6-91/PC",null,"Objímka plochá poloizolovaná, průřez 4-6mm2 / 9,5x1,2mm PC","100ks",12.247124709130787,{"$f":"F740*(1-Elteq!$F$9)","v":12.247124709130787},"8591735011840"]
["TECHNIK","LR 25 T",null,"Letovací plochý kolík mosazný 2,8x0,5mm","100ks",3.265899922434877,{"$f":"F741*(1-Elteq!$F$9)","v":3.265899922434877},"8591735024741"]
["TECHNIK","LR 28",null,"Letovací plochý kolík mosazný 2,8x0,8mm","100ks",2.9318874303676736,{"$f":"F742*(1-Elteq!$F$9)","v":2.9318874303676736},"8591735017316"]
["TECHNIK","LR 45",null,"Letovací plochý kolík mosazný 4,8x0,5mm","100ks",3.6370249136206585,{"$f":"F743*(1-Elteq!$F$9)","v":3.6370249136206585},"8591735024734"]
["TECHNIK","LR 48",null,"Letovací plochý kolík mosazný 4,8x0,8mm","100ks",3.6370249136206585,{"$f":"F744*(1-Elteq!$F$9)","v":3.6370249136206585},"8591735024727"]
["TECHNIK","LR 68 A",null,"Letovací plochý kolík mosazný 6,3x0,8mm / L=17,3mm","100ks",3.5256874162649239,{"$f":"F745*(1-Elteq!$F$9)","v":3.5256874162649239},"8591735052904"]
["TECHNIK","LR 68 K",null,"Letovací plochý kolík mosazný 6,3x0,8mm / L=14,0mm","100ks",3.8968124074507053,{"$f":"F746*(1-Elteq!$F$9)","v":3.8968124074507053},"8591735016067"]
["TECHNIK","LRC 25 T",null,"Letovací plochý kolík cínovaný 2,8x0,5mm","100ks",3.6741374127392366,{"$f":"F747*(1-Elteq!$F$9)","v":3.6741374127392366},"8591735024710"]
["TECHNIK","LRC 28",null,"Letovací plochý kolík cínovaný 2,8x0,8mm","100ks",3.3030124215534551,{"$f":"F748*(1-Elteq!$F$9)","v":3.3030124215534551},"8591735017200"]
["TECHNIK","LRC 28 T",null,"Letovací plochý kolík cínovaný 2,8x0,8mm / trn 1,32x0,8x4,7mm / L=13,7mm","100ks",3.6741374127392366,{"$f":"F749*(1-Elteq!$F$9)","v":3.6741374127392366},"8591735024680"]
["TECHNIK","LRC 45",null,"Letovací plochý kolík cínovaný 4,8x0,5mm","100ks",4.045262403925018,{"$f":"F750*(1-Elteq!$F$9)","v":4.045262403925018},"8591735024697"]
["TECHNIK","LRC 48",null,"Letovací plochý kolík cínovaný 4,8x0,8mm","100ks",4.045262403925018,{"$f":"F751*(1-Elteq!$F$9)","v":4.045262403925018},"8591735017323"]
["TECHNIK","LRC 68 A",null,"Letovací plochý kolík cínovaný 6,3x0,8mm / L=17,3mm","100ks",3.7112499118578146,{"$f":"F752*(1-Elteq!$F$9)","v":3.7112499118578146},"8591735052911"]
["TECHNIK","LRC 68 K",null,"Letovací plochý kolík cínovaný 6,3x0,8mm / L=14,0mm","100ks",4.2679373986364864,{"$f":"F753*(1-Elteq!$F$9)","v":4.2679373986364864},"8591735016074"]
["TECHNIK","LU 28",null,"Letovací plochý kolík zahnutý mosazný 2,8x0,8mm","100ks",2.9689999294862517,{"$f":"F754*(1-Elteq!$F$9)","v":2.9689999294862517},"8591735024703"]
["TECHNIK","LU 68",null,"Letovací plochý kolík zahnutý mosazný 6,3x0,8mm","100ks",3.8968124074507053,{"$f":"F755*(1-Elteq!$F$9)","v":3.8968124074507053},"8591735016081"]
["TECHNIK","LUC 28",null,"Letovací plochý kolík zahnutý cínovaný 2,8x0,8mm","100ks",3.1545624250791424,{"$f":"F756*(1-Elteq!$F$9)","v":3.1545624250791424},"8591735011574"]
["TECHNIK","LUC 68",null,"Letovací plochý kolík zahnutý cínovaný 6,3x0,8mm","100ks",4.2679373986364864,{"$f":"F757*(1-Elteq!$F$9)","v":4.2679373986364864},"8591735017330"]
["TECHNIK","MOLC 68",null,"Mosazná objímka plochá letovací, průřez 6,3x0,8mm cínovaná","100ks",6.4575748466325971,{"$f":"F758*(1-Elteq!$F$9)","v":6.4575748466325971},"8591735014605"]
["TECHNIK","KK 2,5-3,5",null,"Kolík kruhový mosazný, průřez 1,0-2,5mm2 / průměr 3,5mm","100ks",3.8968124074507053,{"$f":"F759*(1-Elteq!$F$9)","v":3.8968124074507053},"8591735033910"]
["TECHNIK","KK 2,5-4",null,"Kolík kruhový mosazný, průřez 1,0-2,5mm2 / průměr 4mm","100ks",3.8968124074507053,{"$f":"F760*(1-Elteq!$F$9)","v":3.8968124074507053},"8591735005993"]
["TECHNIK","KKSN 2,5-3,5",null,"Kolík kruhový mosazný cínovaný, průřez 1,0-2,5mm2 / průměr 3,5mm","100ks",4.045262403925018,{"$f":"F761*(1-Elteq!$F$9)","v":4.045262403925018},"8591735033798"]
["TECHNIK","KKSN 2,5-4",null,"Kolík kruhový mosazný cínovaný, průřez 1,0-2,5mm2 / průměr 4mm","100ks",4.045262403925018,{"$f":"F762*(1-Elteq!$F$9)","v":4.045262403925018},"8591735033712"]
["TECHNIK","KO 2,5-3,5",null,"Kruhová objímka mosazná, průřez 1,0-2,5mm2 / průměr 3,5mm","100ks",3.4514624180277678,{"$f":"F763*(1-Elteq!$F$9)","v":3.4514624180277678},"8591735033903"]
["TECHNIK","KO 2,5-4",null,"Kruhová objímka mosazná, průřez 1,0-2,5mm2 / průměr 4mm","100ks",3.4514624180277678,{"$f":"F764*(1-Elteq!$F$9)","v":3.4514624180277678},"8591735006006"]
["TECHNIK","KOSN 2,5-3,5",null,"Kruhová objímka mosazná cínovaná, průřez 1,0-2,5mm2 / průměr 3,5mm","100ks",3.6370249136206585,{"$f":"F765*(1-Elteq!$F$9)","v":3.6370249136206585},"8591735033781"]
["TECHNIK","KOSN 2,5-4",null,"Kruhová objímka mosazná cínovaná, průřez 1,0-2,5mm2 / průměr 4mm","100ks",3.6370249136206585,{"$f":"F766*(1-Elteq!$F$9)","v":3.6370249136206585},"8591735033705"]
["TECHNIK","MK 1,5-25",null,"Mosazný kolík, průřez 0,5-1,5mm2 / 2,8x0,5mm","100ks",6.1977873528025507,{"$f":"F767*(1-Elteq!$F$9)","v":6.1977873528025507},"8591735006013"]
["TECHNIK","MK 1,5-28",null,"Mosazný kolík, průřez 0,5-1,5mm2 / 2,8x0,8mm","100ks",6.7173623404626444,{"$f":"F768*(1-Elteq!$F$9)","v":6.7173623404626444},"8591735011369"]
["TECHNIK","MK 1,5-45",null,"Mosazný kolík, průřez 0,5-1,5mm2 / 4,8x0,5mm","100ks",3.9339249065692834,{"$f":"F769*(1-Elteq!$F$9)","v":3.9339249065692834},"8591735006020"]
["TECHNIK","MK 1,5-48",null,"Mosazný kolík, průřez 0,5-1,5mm2 / 4,8x0,8mm / síla materiálu 0,8mm","100ks",3.9339249065692834,{"$f":"F770*(1-Elteq!$F$9)","v":3.9339249065692834},"8591735006037"]
["TECHNIK","MK 1,5-68",null,"Mosazný kolík, průřez 0,5-1,5mm2 / 6,3x0,8mm","100ks",4.9359623827708932,{"$f":"F771*(1-Elteq!$F$9)","v":4.9359623827708932},"8591735006044"]
["TECHNIK","MK 1,5-68 P",null,"Mosazný kolík, průřez 0,5-1,5mm2 / 6,3x0,8mm předrolovaný","100ks",4.7503998871780029,{"$f":"F772*(1-Elteq!$F$9)","v":4.7503998871780029},"8591735030551"]
["TECHNIK","MK 2,5-68",null,"Mosazný kolík, průřez 1,5-2,5mm2 / 6,3x0,8mm","100ks",4.4163873951107995,{"$f":"F773*(1-Elteq!$F$9)","v":4.4163873951107995},"8591735006051"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"MK 2,5-68 K",null,"Mosazný kolík, průřez 1,5-2,5mm2 / 6,3x0,8mm krátký","100ks",3.8968124074507053,{"$f":"F774*(1-Elteq!$F$9)","v":3.8968124074507053},"8591735053123"]
["TECHNIK","MK 2,5-68 P",null,"Mosazný kolík, průřez 1,5-2,5mm2 / 6,3x0,8mm předrolovaný","100ks",4.7132873880594248,{"$f":"F775*(1-Elteq!$F$9)","v":4.7132873880594248},"8591735030575"]
["TECHNIK","MK 6-68",null,"Mosazný kolík, průřez 4-6mm2 / 6,3x0,8mm","100ks",6.4946873457511751,{"$f":"F776*(1-Elteq!$F$9)","v":6.4946873457511751},"8591735011116"]
["TECHNIK","MK 6-68 P",null,"Mosazný kolík, průřez 4-6mm2 / 6,3x0,8mm předrolovaný","100ks",5.641099866023878,{"$f":"F777*(1-Elteq!$F$9)","v":5.641099866023878},"8591735030582"]
["TECHNIK","MKC 1,5-25",null,"Mosazný kolík cínovaný, průřez 0,5-1,5mm2 / 2,8x0,5mm","100ks",6.8286998378183785,{"$f":"F778*(1-Elteq!$F$9)","v":6.8286998378183785},"8591735006075"]
["TECHNIK","MKC 1,5-28",null,"Mosazný kolík cínovaný, průřez 0,5-1,5mm2 / 2,8x0,8mm","100ks",7.0884873316484258,{"$f":"F779*(1-Elteq!$F$9)","v":7.0884873316484258},"8591735006099"]
["TECHNIK","MKC 1,5-45",null,"Mosazný kolík cínovaný, průřez 0,5-1,5mm2 / 4,8x0,5mm","100ks",4.3421623968736434,{"$f":"F780*(1-Elteq!$F$9)","v":4.3421623968736434},"8591735006105"]
["TECHNIK","MKC 1,5-48",null,"Mosazný kolík cínovaný, průřez 0,5-1,5mm2 / 4,8x0,8mm / síla materiálu 0,4mm","100ks",7.0884873316484258,{"$f":"F781*(1-Elteq!$F$9)","v":7.0884873316484258},"8591735006112"]
["TECHNIK","MKC 1,5-68",null,"Mosazný kolík cínovaný, průřez 0,5-1,5mm2 / 6,3x0,8mm","100ks",5.3813123721938307,{"$f":"F782*(1-Elteq!$F$9)","v":5.3813123721938307},"8591735006129"]
["TECHNIK","MKC 1,5-68 P",null,"Mosazný kolík cínovaný, průřez 0,5-1,5mm2 / 6,3x0,8mm předrolovaný","100ks",5.1957498766009405,{"$f":"F783*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735015954"]
["TECHNIK","MKC 2,5-68 ",null,"Mosazný kolík cínovaný, průřez 1,5-2,5mm2 / 6,3x0,8mm","100ks",4.7875123862965809,{"$f":"F784*(1-Elteq!$F$9)","v":4.7875123862965809},"8591735005672"]
["TECHNIK","MKC 2,5-68 K",null,"Mosazný kolík cínovaný, průřez 1,5-2,5mm2 / 6,3x0,8mm krátký","100ks",4.2679373986364864,{"$f":"F785*(1-Elteq!$F$9)","v":4.2679373986364864},"8591735053130"]
["TECHNIK","MKC 2,5-68 P",null,"Mosazný kolík cínovaný, průřez 1,5-2,5mm2 / 6,3x0,8mm předrolovaný","100ks",5.1586373774823624,{"$f":"F786*(1-Elteq!$F$9)","v":5.1586373774823624},"8591735015961"]
["TECHNIK","MKC 6-68",null,"Mosazný kolík cínovaný, průřez 4-6mm2 / 6,3x0,8mm","100ks",8.053412308731458,{"$f":"F787*(1-Elteq!$F$9)","v":8.053412308731458},"8591735052157"]
["TECHNIK","MKC 6-68 P",null,"Mosazný kolík cínovaný, průřez 4-6mm2 / 6,3x0,8mm předrolovaný","100ks",7.4596123228342073,{"$f":"F788*(1-Elteq!$F$9)","v":7.4596123228342073},"8591735015978"]
["TECHNIK","MKJ 1,5-25",null,"Mosazný kolík s jazýčkem, průřez 0,5-1,5mm2 / 2,8x0,5mm","100ks",6.6060248431069102,{"$f":"F789*(1-Elteq!$F$9)","v":6.6060248431069102},"8591735034290"]
["TECHNIK","MKJ 1,5-28",null,"Mosazný kolík s jazýčkem, průřez 0,5-1,5mm2 / 2,8x0,8mm","100ks",7.0142623334112697,{"$f":"F790*(1-Elteq!$F$9)","v":7.0142623334112697},"8591735006143"]
["TECHNIK","MKJ 1,5-68",null,"Mosazný kolík s jazýčkem, průřez 0,5-1,5mm2 / 6,3x0,8mm","100ks",2.9318874303676736,{"$f":"F791*(1-Elteq!$F$9)","v":2.9318874303676736},"8591735006150"]
["TECHNIK","MKJ 2,5-55",null,"Mosazný kolík s jazýčkem, průřez 1,5-2,5mm2 / 5,5x0,8mm","100ks",14.102749665059696,{"$f":"F792*(1-Elteq!$F$9)","v":14.102749665059696},"8591735046392"]
["TECHNIK","MKJ 2,5-68",null,"Mosazný kolík s jazýčkem, průřez 1,5-2,5mm2 / 6,3x0,8mm","100ks",3.0432249277234078,{"$f":"F793*(1-Elteq!$F$9)","v":3.0432249277234078},"8591735006167"]
["TECHNIK","MKJ 2,5-68 P",null,"Mosazný kolík s jazýčkem, průřez 1,5-2,5mm2 / 6,3x0,8mm předrolovaný","100ks",3.7483624109763927,{"$f":"F794*(1-Elteq!$F$9)","v":3.7483624109763927},"8591735030599"]
["TECHNIK","MKJ 6-68",null,"Mosazný kolík s jazýčkem, průřez 4,0-6,0mm2 / 6,3x0,8mm","100ks",8.6472122946287087,{"$f":"F795*(1-Elteq!$F$9)","v":8.6472122946287087},"8591735011123"]
["TECHNIK","MKJC 1,5-25",null,"Mosazný kolík s jazýčkem, průřez 0,5-1,5mm2 / 2,8x0,5mm","100ks",7.7936248149014107,{"$f":"F796*(1-Elteq!$F$9)","v":7.7936248149014107},"8591735015947"]
["TECHNIK","MKJC 1,5-28",null,"Mosazný kolík s jazýčkem, průřez 0,5-1,5mm2 / 2,8x0,8mm","100ks",10.985299739099132,{"$f":"F797*(1-Elteq!$F$9)","v":10.985299739099132},"8591735006174"]
["TECHNIK","MKJC 1,5-48",null,"Mosazný kolík s jazýčkem, průřez 0,5-1,5mm2 / 4,8x0,8mm","100ks",10.465724751439037,{"$f":"F798*(1-Elteq!$F$9)","v":10.465724751439037},"8591735019549"]
["TECHNIK","MKJC 1,5-68",null,"Mosazný kolík s jazýčkem, průřez 0,5-1,5mm2 / 6,3x0,8mm","100ks",3.4885749171463458,{"$f":"F799*(1-Elteq!$F$9)","v":3.4885749171463458},"8591735006181"]
["TECHNIK","MKJC 1,5-68 P",null,"Mosazný kolík s jazýčkem, průřez 0,5-1,5mm2 / 6,3x0,8mm předrolovaný","100ks",6.1235623545653937,{"$f":"F800*(1-Elteq!$F$9)","v":6.1235623545653937},"8591735055196"]
["TECHNIK","MKJC 2,5-68",null,"Mosazný kolík s jazýčkem, průřez 1,5-2,5mm2 / 6,3x0,8mm","100ks",3.5256874162649239,{"$f":"F801*(1-Elteq!$F$9)","v":3.5256874162649239},"8591735006198"]
["TECHNIK","MKJC 2,5-68 P",null,"Mosazný kolík s jazýčkem, průřez 1,5-2,5mm2 / 6,3x0,8mm předrolovaný","100ks",4.1937124003993302,{"$f":"F802*(1-Elteq!$F$9)","v":4.1937124003993302},"8591735030605"]
["TECHNIK","MKJC 6-68",null,"Mosazný kolík s jazýčkem, průřez 4-6mm2 / 6,3x0,8mm","100ks",9.4265747761188496,{"$f":"F803*(1-Elteq!$F$9)","v":9.4265747761188496},"8591735006204"]
["TECHNIK","MKJC 6-68 P",null,"Mosazný kolík s jazýčkem, průřez 4-6mm2 / 6,3x0,8mm předrolovaný","100ks",14.21408716241543,{"$f":"F804*(1-Elteq!$F$9)","v":14.21408716241543},"8591735055394"]
["TECHNIK","MO 0,25-25",null,"Mosazná objímka, průřez 0,1-0,25mm2 / 2,8x0,5mm","100ks",1.4844999647431258,{"$f":"F805*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735006211"]
["TECHNIK","MO 0,25-28",null,"Mosazná objímka, průřez 0,1-0,25mm2 / 2,8x0,8mm","100ks",1.4844999647431258,{"$f":"F806*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735006228"]
["TECHNIK","MO 0,5-25",null,"Mosazná objímka, průřez 0,25-0,5mm2 / 2,8x0,5mm","100ks",1.4844999647431258,{"$f":"F807*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735006235"]
["TECHNIK","MO 0,5-28",null,"Mosazná objímka, průřez 0,25-0,5mm2 / 2,8x0,8mm","100ks",1.4844999647431258,{"$f":"F808*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735006242"]
["TECHNIK","MO 1,5-25",null,"Mosazná objímka, průřez 0,5-1,0mm2 / 2,8x0,5mm","100ks",1.5587249629802822,{"$f":"F809*(1-Elteq!$F$9)","v":1.5587249629802822},"8591735006266"]
["TECHNIK","MO 1,5-25 K",null,"Mosazná objímka, průřez 0,5-1,5mm2 / 2,8x0,5mm bez zářezů","100ks",1.4844999647431258,{"$f":"F810*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735053147"]
["TECHNIK","MO 1,5-28",null,"Mosazná objímka, průřez 0,5-1,0mm2 / 2,8x0,8mm","100ks",1.5587249629802822,{"$f":"F811*(1-Elteq!$F$9)","v":1.5587249629802822},"8591735006273"]
["TECHNIK","MO 1,5-28 K",null,"Mosazná objímka, průřez 0,5-1,5mm2 / 2,8x0,8mm bez zářezů","100ks",1.4844999647431258,{"$f":"F812*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735053154"]
["TECHNIK","MO 1,5-45",null,"Mosazná objímka, průřez 0,5-1,5mm2 / 4,8x0,5mm","100ks",2.1154124497589541,{"$f":"F813*(1-Elteq!$F$9)","v":2.1154124497589541},"8591735006280"]
["TECHNIK","MO 1,5-45 P",null,"Mosazná objímka, průřez 0,5-1,5mm2 / 4,8x0,5mm předrolovaná","100ks",2.2267499471146888,{"$f":"F814*(1-Elteq!$F$9)","v":2.2267499471146888},"8591735056704"]
["TECHNIK","MO 1,5-48",null,"Mosazná objímka, průřez 0,5-1,5mm2 / 4,8x0,8mm","100ks",2.1154124497589541,{"$f":"F815*(1-Elteq!$F$9)","v":2.1154124497589541},"8591735006297"]
["TECHNIK","MO 1,5-48 BP",null,"Mosazná objímka, průřez 0,5-1,5mm2 / 4,8x0,8mm, s bočním připojením typ A","100ks",6.9400373351741136,{"$f":"F816*(1-Elteq!$F$9)","v":6.9400373351741136},"8591735013288"]
["TECHNIK","MO 1,5-48 BP-B",null,"Mosazná objímka, průřez 0,5-1,5mm2 / 4,8x0,8mm, s bočním připojením typ B","100ks",4.00814990480644,{"$f":"F817*(1-Elteq!$F$9)","v":4.00814990480644},"8591735032135"]
["TECHNIK","MO 1,5-48 P",null,"Mosazná objímka, průřez 0,5-1,5mm2 / 4,8x0,8mm předrolovaná","100ks",2.2267499471146888,{"$f":"F818*(1-Elteq!$F$9)","v":2.2267499471146888},"8591735056698"]
["TECHNIK","MO 1,5-68",null,"Mosazná objímka, průřez 0,5-1,5mm2 / 6,3x0,8mm","100ks",2.5236499400633141,{"$f":"F819*(1-Elteq!$F$9)","v":2.5236499400633141},"8591735005986"]
["TECHNIK","MO 1,5-68 BP",null,"Mosazná objímka, průřez 0,5-1,5mm2 / 6,3x0,8mm, s bočním připojením typ A","100ks",2.8576624321305171,{"$f":"F820*(1-Elteq!$F$9)","v":2.8576624321305171},"8591735014018"]
["TECHNIK","MO 1,5-68 BP-B",null,"Mosazná objímka, průřez 0,5-1,5mm2 / 6,3x0,8mm, s bočním připojením typ B","100ks",6.1977873528025507,{"$f":"F821*(1-Elteq!$F$9)","v":6.1977873528025507},"8591735054694"]
["TECHNIK","MO 1,5-68 P",null,"Mosazná objímka, průřez 0,5-1,5mm2 / 6,3x0,8mm předrolovaná","100ks",3.3772374197906112,{"$f":"F822*(1-Elteq!$F$9)","v":3.3772374197906112},"8591735027155"]
["TECHNIK","MO 2,5-45",null,"Mosazná objímka, průřez 1,5-2,5mm2 / 4,8x0,5mm","100ks",5.5297623686681439,{"$f":"F823*(1-Elteq!$F$9)","v":5.5297623686681439},"8591735011376"]
["TECHNIK","MO 2,5-48",null,"Mosazná objímka, průřez 1,5-2,5mm2 / 4,8x0,8mm","100ks",5.5297623686681439,{"$f":"F824*(1-Elteq!$F$9)","v":5.5297623686681439},"8591735011383"]
["TECHNIK","MO 2,5-68",null,"Mosazná objímka, průřez 1,5-2,5mm2 / 6,3x0,8mm","100ks",2.5236499400633141,{"$f":"F825*(1-Elteq!$F$9)","v":2.5236499400633141},"8591735006303"]
["TECHNIK","MO 2,5-68 BP",null,"Mosazná objímka, průřez 1,5-2,5mm2 / 6,3x0,8mm, s bočním připojením typ A","100ks",3.1545624250791424,{"$f":"F826*(1-Elteq!$F$9)","v":3.1545624250791424},"8591735006310"]
["TECHNIK","MO 2,5-68 BP-B",null,"Mosazná objímka, průřez 1,5-2,5mm2 / 6,3x0,8mm, s bočním připojením typ B","100ks",5.641099866023878,{"$f":"F827*(1-Elteq!$F$9)","v":5.641099866023878},"8591735054717"]
["TECHNIK","MO 2,5-68 P",null,"Mosazná objímka, průřez 1,5-2,5mm2 / 6,3x0,8mm předrolovaná","100ks",3.4885749171463458,{"$f":"F828*(1-Elteq!$F$9)","v":3.4885749171463458},"8591735030612"]
["TECHNIK","MO 6-68",null,"Mosazná objímka, průřez 4,0-6,0mm2 / 6,3x0,8mm","100ks",2.9689999294862517,{"$f":"F829*(1-Elteq!$F$9)","v":2.9689999294862517},"8591735006334"]
["TECHNIK","MO 6-68 P",null,"Mosazná objímka, průřez 4-6mm2 / 6,3x0,8mm předrolovaná","100ks",3.7112499118578146,{"$f":"F830*(1-Elteq!$F$9)","v":3.7112499118578146},"8591735030629"]
["TECHNIK","MO 6-91",null,"Mosazná objímka, průřez 4,0-6,0mm2 / 9,5x1,2mm předrolovaná","100ks",9.2038997814073795,{"$f":"F831*(1-Elteq!$F$9)","v":9.2038997814073795},"8591735006341"]
["TECHNIK","MOC 0,25-25",null,"Mosazná objímka cínovaná, průřez 0,1-0,25mm2 / 2,8x0,5mm","100ks",1.6700624603360166,{"$f":"F832*(1-Elteq!$F$9)","v":1.6700624603360166},"8591735006358"]
["TECHNIK","MOC 0,25-28",null,"Mosazná objímka cínovaná, průřez 0,1-0,25mm2 / 2,8x0,8mm","100ks",1.6700624603360166,{"$f":"F833*(1-Elteq!$F$9)","v":1.6700624603360166},"8591735006365"]
["TECHNIK","MOC 0,5-25",null,"Mosazná objímka cínovaná, průřez 0,25-0,5mm2 / 2,8x0,5mm","100ks",1.6700624603360166,{"$f":"F834*(1-Elteq!$F$9)","v":1.6700624603360166},"8591735006372"]
["TECHNIK","MOC 0,5-28",null,"Mosazná objímka cínovaná, průřez 0,25-0,5mm2 / 2,8x0,8mm","100ks",1.6700624603360166,{"$f":"F835*(1-Elteq!$F$9)","v":1.6700624603360166},"8591735006389"]
["TECHNIK","MOC 1,0-28",null,"Mosazná objímka cínovaná, průřez 0,35-1,0mm2 / 2,8x0,8mm","100ks",3.5256874162649239,{"$f":"F836*(1-Elteq!$F$9)","v":3.5256874162649239},"8591735056797"]
["TECHNIK","MOC 1,5-25",null,"Mosazná objímka cínovaná, průřez 0,5-1,0mm2 / 2,8x0,5mm","100ks",1.7442874585731729,{"$f":"F837*(1-Elteq!$F$9)","v":1.7442874585731729},"8591735006402"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"MOC 1,5-25 K",null,"Mosazná objímka cínovaná, průřez 0,5-1,5mm2 / 2,8x0,5mm bez zářezů","100ks",1.6700624603360166,{"$f":"F838*(1-Elteq!$F$9)","v":1.6700624603360166},"8591735053161"]
["TECHNIK","MOC 1,5-28",null,"Mosazná objímka cínovaná, průřez 0,5-1,0mm2 / 2,8x0,8mm","100ks",1.7442874585731729,{"$f":"F839*(1-Elteq!$F$9)","v":1.7442874585731729},"8591735006419"]
["TECHNIK","MOC 1,5-28 K",null,"Mosazná objímka cínovaná, průřez 0,5-1,5mm2 / 2,8x0,8mm bez zářezů","100ks",1.6700624603360166,{"$f":"F840*(1-Elteq!$F$9)","v":1.6700624603360166},"8591735053178"]
["TECHNIK","MOC 1,5-45",null,"Mosazná objímka cínovaná, průřez 0,5-1,5mm2 / 4,8x0,5mm","100ks",2.3009749453518449,{"$f":"F841*(1-Elteq!$F$9)","v":2.3009749453518449},"8591735056681"]
["TECHNIK","MOC 1,5-45 P",null,"Mosazná objímka cínovaná, průřez 0,5-1,5mm2 / 4,8x0,5mm předrolovaná","100ks",2.4123124427075795,{"$f":"F842*(1-Elteq!$F$9)","v":2.4123124427075795},"8591735005979"]
["TECHNIK","MOC 1,5-48",null,"Mosazná objímka cínovaná, průřez 0,5-1,5mm2 / 4,8x0,8mm","100ks",2.3009749453518449,{"$f":"F843*(1-Elteq!$F$9)","v":2.3009749453518449},"8591735006426"]
["TECHNIK","MOC 1,5-48 BP",null,"Mosazná objímka cínovaná, průřez 0,5-1,5mm2 / 4,8x0,8mm, s bočním připojením typ A","100ks",7.311162326359895,{"$f":"F844*(1-Elteq!$F$9)","v":7.311162326359895},"8591735016005"]
["TECHNIK","MOC 1,5-48 BP-B",null,"Mosazná objímka cínovaná, průřez 0,5-1,5mm2 / 4,8x0,8mm, s bočním připojením typ B","100ks",4.4906123933479556,{"$f":"F845*(1-Elteq!$F$9)","v":4.4906123933479556},"8591735055202"]
["TECHNIK","MOC 1,5-48 P",null,"Mosazná objímka cínovaná, průřez 0,5-1,5mm2 / 4,8x0,8mm předrolovaná","100ks",2.4123124427075795,{"$f":"F846*(1-Elteq!$F$9)","v":2.4123124427075795},"8591735056674"]
["TECHNIK","MOC 1,5-48/IMP",null,"Mosazná objímka cínovaná, průřez 0,5-1,5mm2 / 4,8x0,8mm (MOQ 5000ks)","100ks",2.3009749453518449,{"$f":"F847*(1-Elteq!$F$9)","v":2.3009749453518449},"8591735029340"]
["TECHNIK","MOC 1,5-68",null,"Mosazná objímka cínovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm","100ks",2.9318874303676736,{"$f":"F848*(1-Elteq!$F$9)","v":2.9318874303676736},"8591735006433"]
["TECHNIK","MOC 1,5-68 BP",null,"Mosazná objímka cínovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm, s bočním připojením typ A","100ks",3.0803374268419863,{"$f":"F849*(1-Elteq!$F$9)","v":3.0803374268419863},"8591735010805"]
["TECHNIK","MOC 1,5-68 BP-B",null,"Mosazná objímka cínovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm, s bočním připojením typ B","100ks",6.8658123369369566,{"$f":"F850*(1-Elteq!$F$9)","v":6.8658123369369566},"8591735054700"]
["TECHNIK","MOC 1,5-68 BP-B P",null,"Mosazná objímka cínovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm, s bočním připojením typ B předrolovaný","100ks",8.053412308731458,{"$f":"F851*(1-Elteq!$F$9)","v":8.053412308731458},"8591735024109"]
["TECHNIK","MOC 1,5-68 J",null,"Mosazná objímka cínovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm JST","100ks",4.4906123933479556,{"$f":"F852*(1-Elteq!$F$9)","v":4.4906123933479556},"8591735029197"]
["TECHNIK","MOC 1,5-68 MX",null,"Mosazná objímka cínovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm","100ks",2.9318874303676736,{"$f":"F853*(1-Elteq!$F$9)","v":2.9318874303676736},"8591735013455"]
["TECHNIK","MOC 1,5-68 P",null,"Mosazná objímka cínovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm předrolovaná","100ks",3.59991241450208,{"$f":"F854*(1-Elteq!$F$9)","v":3.59991241450208},"8591735016012"]
["TECHNIK","MOC 2,5-45",null,"Mosazná objímka cínovaná, průřez 1,5-2,5mm2 / 4,8x0,5mm","100ks",6.9771498342926916,{"$f":"F855*(1-Elteq!$F$9)","v":6.9771498342926916},"8591735006440"]
["TECHNIK","MOC 2,5-48",null,"Mosazná objímka cínovaná, průřez 1,5-2,5mm2 / 4,8x0,8mm","100ks",6.9771498342926916,{"$f":"F856*(1-Elteq!$F$9)","v":6.9771498342926916},"8591735006457"]
["TECHNIK","MOC 2,5-68",null,"Mosazná objímka cínovaná, průřez 1,5-2,5mm2 / 6,3x0,8mm","100ks",3.3030124215534551,{"$f":"F857*(1-Elteq!$F$9)","v":3.3030124215534551},"8591735006464"]
["TECHNIK","MOC 2,5-68 BP",null,"Mosazná objímka cínovaná, průřez 0,5-2,5mm2 / 6,3x0,8mm, s bočním připojením","100ks",3.8225874092135492,{"$f":"F858*(1-Elteq!$F$9)","v":3.8225874092135492},"8591735010799"]
["TECHNIK","MOC 2,5-68 BP MX",null,"Mosazná objímka cínovaná, průřez 1,5-2,5mm2 / 6,3x0,8mm, s bočním připojením","100ks",4.4906123933479556,{"$f":"F859*(1-Elteq!$F$9)","v":4.4906123933479556},"8591735015479"]
["TECHNIK","MOC 2,5-68 BP-B",null,"Mosazná objímka cínovaná, průřez 1,5-2,5mm2 / 6,3x0,8mm, s bočním připojením typ B","100ks",6.2348998519211287,{"$f":"F860*(1-Elteq!$F$9)","v":6.2348998519211287},"8591735054724"]
["TECHNIK","MOC 2,5-68 P",null,"Mosazná objímka cínovaná, průřez 1,5-2,5mm2 / 6,3x0,8mm předrolovaná","100ks",3.7483624109763927,{"$f":"F861*(1-Elteq!$F$9)","v":3.7483624109763927},"8591735016029"]
["TECHNIK","MOC 3900-0039",null,"Mosazná objímka cínovaná","100ks",9.4265747761188496,{"$f":"F862*(1-Elteq!$F$9)","v":9.4265747761188496},""]
["TECHNIK","MOC 6-68",null,"Mosazná objímka cínovaná, průřez 4-6mm2 / 6,3x0,8mm","100ks",3.3401249206720331,{"$f":"F863*(1-Elteq!$F$9)","v":3.3401249206720331},"8591735006488"]
["TECHNIK","MOC 6-68 P",null,"Mosazná objímka cínovaná, průřez 4-6mm2 / 6,3x0,8mm předrolovaná","100ks",4.00814990480644,{"$f":"F864*(1-Elteq!$F$9)","v":4.00814990480644},"8591735016036"]
["TECHNIK","MOC 6-91",null,"Mosazná objímka cínovaná, průřez 4-6mm2 / 9,5x1,2mm předrolovaná","100ks",9.6121372717117399,{"$f":"F865*(1-Elteq!$F$9)","v":9.6121372717117399},"8591735006495"]
["TECHNIK","MOJ 1,5-25",null,"Mosazná objímka s jazýčkem, průřez 0,5-1,0mm2 / 2,8x0,5mm","100ks",3.4885749171463458,{"$f":"F866*(1-Elteq!$F$9)","v":3.4885749171463458},"8591735033637"]
["TECHNIK","MOJ 1,5-28",null,"Mosazná objímka s jazýčkem, průřez 0,5-1,0mm2 / 2,8x0,8mm","100ks",3.4885749171463458,{"$f":"F867*(1-Elteq!$F$9)","v":3.4885749171463458},"8591735015527"]
["TECHNIK","MOJ 1,5-48",null,"Mosazná objímka s jazýčkem, průřez 0,5-1,5mm2 / 4,8x0,8mm","100ks",7.6451748184270985,{"$f":"F868*(1-Elteq!$F$9)","v":7.6451748184270985},"8591735021320"]
["TECHNIK","MOJ 1,5-68",null,"Mosazná objímka s jazýčkem, průřez 0,5-1,5mm2 / 6,3x0,8mm","100ks",2.4123124427075795,{"$f":"F869*(1-Elteq!$F$9)","v":2.4123124427075795},"8591735006501"]
["TECHNIK","MOJ 1,5-68 P",null,"Mosazná objímka s jazýčkem, průřez 0,5-1,5mm2 / 6,3x0,8mm předrolovaná","100ks",3.7854749100949707,{"$f":"F870*(1-Elteq!$F$9)","v":3.7854749100949707},"8591735030636"]
["TECHNIK","MOJ 2,5-48",null,"Mosazná objímka s jazýčkem, průřez 1,5-2,5mm2 / 4,8x0,8mm","100ks",7.6451748184270985,{"$f":"F871*(1-Elteq!$F$9)","v":7.6451748184270985},"8591735017811"]
["TECHNIK","MOJ 2,5-55",null,"Mosazná objímka s jazýčkem, průřez 1,5-2,5mm2 / 5,5x0,8mm","100ks",11.133749735573444,{"$f":"F872*(1-Elteq!$F$9)","v":11.133749735573444},"8591735042042"]
["TECHNIK","MOJ 2,5-68",null,"Mosazná objímka s jazýčkem, průřez 1,5-2,5mm2 / 6,3x0,8mm","100ks",2.5607624391818922,{"$f":"F873*(1-Elteq!$F$9)","v":2.5607624391818922},"8591735006518"]
["TECHNIK","MOJ 2,5-68 P",null,"Mosazná objímka s jazýčkem, průřez 1,5-2,5mm2 / 6,3x0,8mm předrolovaná","100ks",3.9339249065692834,{"$f":"F874*(1-Elteq!$F$9)","v":3.9339249065692834},"8591735030643"]
["TECHNIK","MOJ 2,5-88 BP",null,"Mosazná objímka s jazýčkem, průřez 1,5-2,5mm2 / 7,7x0,8mm, s bočním připojením","100ks",3.8968124074507053,{"$f":"F875*(1-Elteq!$F$9)","v":3.8968124074507053},"8591735015992"]
["TECHNIK","MOJ 6-68",null,"Mosazná objímka s jazýčkem, průřez 4-6mm2 / 6,3x0,8mm","100ks",6.1606748536839726,{"$f":"F876*(1-Elteq!$F$9)","v":6.1606748536839726},"8591735011390"]
["TECHNIK","MOJ 6-68 P",null,"Mosazná objímka s jazýčkem, průřez 4-6mm2 / 6,3x0,8mm předrolovaná","100ks",4.2308248995179083,{"$f":"F877*(1-Elteq!$F$9)","v":4.2308248995179083},"8591735030650"]
["TECHNIK","MOJC 1,5-25",null,"Mosazná objímka s jazýčkem cínovaná, průřez 0,5-1,0mm2 / 2,8x0,5mm","100ks",3.8968124074507053,{"$f":"F878*(1-Elteq!$F$9)","v":3.8968124074507053},"8591735019082"]
["TECHNIK","MOJC 1,5-28",null,"Mosazná objímka s jazýčkem cínovaná, průřez 0,5-1,0mm2 / 2,8x0,8mm","100ks",3.8968124074507053,{"$f":"F879*(1-Elteq!$F$9)","v":3.8968124074507053},"8591735015596"]
["TECHNIK","MOJC 1,5-48",null,"Mosazná objímka s jazýčkem cínovaná, průřez 0,5-1,5mm2 / 4,8x0,8mm","100ks",7.7936248149014107,{"$f":"F880*(1-Elteq!$F$9)","v":7.7936248149014107},"8591735019556"]
["TECHNIK","MOJC 1,5-68",null,"Mosazná objímka s jazýčkem cínovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm","100ks",2.8947749312490956,{"$f":"F881*(1-Elteq!$F$9)","v":2.8947749312490956},"8591735006525"]
["TECHNIK","MOJC 1,5-68 BP",null,"Mosazná objímka s jazýčkem cínovaná, průřez 0,5-1,0mm2 / 6,3x0,8mm s bočním připojením","100ks",28.391061825712281,{"$f":"F882*(1-Elteq!$F$9)","v":28.391061825712281},"8591735036386"]
["TECHNIK","MOJC 1,5-68 P",null,"Mosazná objímka s jazýčkem cínovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm předrolovaná","100ks",4.00814990480644,{"$f":"F883*(1-Elteq!$F$9)","v":4.00814990480644},"8591735030667"]
["TECHNIK","MOJC 2,5-48",null,"Mosazná objímka s jazýčkem cínovaná, průřez 1,5-2,5mm2 / 4,8x0,8mm","100ks",7.7936248149014107,{"$f":"F884*(1-Elteq!$F$9)","v":7.7936248149014107},"8591735025526"]
["TECHNIK","MOJC 2,5-68",null,"Mosazná objímka s jazýčkem cínovaná, průřez 1,5-2,5mm2 / 6,3x0,8mm","100ks",2.9689999294862517,{"$f":"F885*(1-Elteq!$F$9)","v":2.9689999294862517},"8591735006532"]
["TECHNIK","MOJC 2,5-68 P",null,"Mosazná objímka s jazýčkem cínovaná, průřez 1,5-2,5mm2 / 6,3x0,8mm předrolovaná","100ks",4.1937124003993302,{"$f":"F886*(1-Elteq!$F$9)","v":4.1937124003993302},"8591735030674"]
["TECHNIK","MOJC 6-68",null,"Mosazná objímka s jazýčkem cínovaná, průřez 4-6mm2 / 6,3x0,8mm","100ks",7.3482748254784731,{"$f":"F887*(1-Elteq!$F$9)","v":7.3482748254784731},"8591735006549"]
["TECHNIK","MOJC 6-68 P",null,"Mosazná objímka s jazýčkem cínovaná, průřez 4-6mm2 / 6,3x0,8mm předrolovaná","100ks",5.1215248783637843,{"$f":"F888*(1-Elteq!$F$9)","v":5.1215248783637843},"8591735023119"]
["TECHNIK","MOO 1,5-48",null,"Mosazná objímka odbočná, průřez 0,5-1,5mm2 / 4,8x0,8mm (MOQ 3000ks)","100ks",8.4987622981543947,{"$f":"F889*(1-Elteq!$F$9)","v":8.4987622981543947},"8591735011406"]
["TECHNIK","MOO 1,5-68",null,"Mosazná objímka odbočná, průřez 0,5-1,5mm2 / 6,3x0,8mm","100ks",5.8266623616167692,{"$f":"F890*(1-Elteq!$F$9)","v":5.8266623616167692},"8591735006556"]
["TECHNIK","MOO 1,5-68 P",null,"Mosazná objímka odbočná, průřez 0,5-1,5mm2 / 6,3x0,8mm předrolovaná","100ks",6.3462373492768629,{"$f":"F891*(1-Elteq!$F$9)","v":6.3462373492768629},"8591735014346"]
["TECHNIK","MOO 2,5-48",null,"Mosazná objímka odbočná, průřez 1,5-2,5mm2 / 4,8x0,8mm","100ks",10.725512245269083,{"$f":"F892*(1-Elteq!$F$9)","v":10.725512245269083},"8591735011413"]
["TECHNIK","MOO 2,5-68",null,"Mosazná objímka odbočná, průřez 1,5-2,5mm2 / 6,3x0,8mm","100ks",5.8637748607353473,{"$f":"F893*(1-Elteq!$F$9)","v":5.8637748607353473},"8591735006563"]
["TECHNIK","MOO 2,5-68 P",null,"Mosazná objímka odbočná, průřez 1,5-2,5mm2 / 6,3x0,8mm předrolovaná","100ks",6.4946873457511751,{"$f":"F894*(1-Elteq!$F$9)","v":6.4946873457511751},"8591735053093"]
["TECHNIK","MOOC 1,5-48",null,"Mosazná objímka odbočná cínovaná, průřez 0,5-1,5mm2 / 4,8x0,8mm","100ks",9.5750247725931619,{"$f":"F895*(1-Elteq!$F$9)","v":9.5750247725931619},"8591735006587"]
["TECHNIK","MOOC 1,5-68",null,"Mosazná objímka odbočná cínovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm","100ks",6.0493373563282375,{"$f":"F896*(1-Elteq!$F$9)","v":6.0493373563282375},"8591735006594"]
["TECHNIK","MOOC 1,5-68 P",null,"Mosazná objímka odbočná cínovaná, průřez 0,5-1,5mm2 / 6,3x0,8mm předrolovaná","100ks",6.7173623404626444,{"$f":"F897*(1-Elteq!$F$9)","v":6.7173623404626444},"8591735053109"]
["TECHNIK","MOOC 2,5-48",null,"Mosazná objímka odbočná cínovaná, průřez 1,5-2,5mm2 / 4,8x0,8mm předrolovaná","100ks",10.725512245269083,{"$f":"F898*(1-Elteq!$F$9)","v":10.725512245269083},"8591735006600"]
["TECHNIK","MOOC 2,5-68",null,"Mosazná objímka odbočná cínovaná, průřez 1,5-2,5mm2 / 6,3x0,8mm","100ks",6.5689123439883321,{"$f":"F899*(1-Elteq!$F$9)","v":6.5689123439883321},"8591735006617"]
["TECHNIK","MOOC 2,5-68 P",null,"Mosazná objímka odbočná cínovaná, průřez 1,5-2,5mm2 / 6,3x0,8mm předrolovaná","100ks",6.8658123369369566,{"$f":"F900*(1-Elteq!$F$9)","v":6.8658123369369566},"8591735053116"]
["TECHNIK","OON 1,0-68",null,"Ocelová objímka niklovaná 0,5-1,0mm2 / 6,3x0,8mm","100ks",3.8225874092135492,{"$f":"F901*(1-Elteq!$F$9)","v":3.8225874092135492},"8591735006624"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"OON 2,5-68",null,"Ocelová objímka niklovaná 1,0-2,5mm2 / 6,3x0,8mm","100ks",4.0823749030435961,{"$f":"F902*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735006631"]
["TECHNIK","OON 6-68",null,"Ocelová objímka niklovaná 4-6mm2 / 6,3x0,8mm","100ks",4.5648373915851117,{"$f":"F903*(1-Elteq!$F$9)","v":4.5648373915851117},"8591735004354"]
["TECHNIK","ND 68-M2,5",null,"Nýtovací plochý kolík mosazný, rozměr 6,3x0,8mm / M2,5 / 45°","100ks",4.1565999012807522,{"$f":"F904*(1-Elteq!$F$9)","v":4.1565999012807522},"8591735006648"]
["TECHNIK","ND 68-M3",null,"Nýtovací plochý kolík mosazný, rozměr 6,3x0,8mm / M3 / 45°","100ks",4.1565999012807522,{"$f":"F905*(1-Elteq!$F$9)","v":4.1565999012807522},"8591735006655"]
["TECHNIK","ND 68-M4",null,"Nýtovací plochý kolík mosazný, rozměr 6,3x0,8mm / M4 / 45°","100ks",4.1565999012807522,{"$f":"F906*(1-Elteq!$F$9)","v":4.1565999012807522},"8591735006662"]
["TECHNIK","ND 68-M4/5000",null,"Nýtovací plochý kolík mosazný, rozměr 6,3x0,8mm / M4 / 45° (MOQ 5000ks)","5000ks",201.70643270947221,{"$f":"F907*(1-Elteq!$F$9)","v":201.70643270947221},"8591735050191"]
["TECHNIK","ND 68-M4-90",null,"Nýtovací plochý kolík mosazný, rozměr 6,3x0,8mm / M4 / 90°","100ks",4.6761748889408468,{"$f":"F908*(1-Elteq!$F$9)","v":4.6761748889408468},""]
["TECHNIK","ND 68-M5",null,"Nýtovací plochý kolík mosazný, rozměr 6,3x0,8mm / M5 / 45°","100ks",4.1565999012807522,{"$f":"F909*(1-Elteq!$F$9)","v":4.1565999012807522},"8591735006679"]
["TECHNIK","ND 68-M5-90",null,"Nýtovací plochý kolík mosazný, rozměr 6,3x0,8mm / M5 / 90°","100ks",4.6761748889408468,{"$f":"F910*(1-Elteq!$F$9)","v":4.6761748889408468},""]
["TECHNIK","ND 68-M6",null,"Nýtovací plochý kolík mosazný, rozměr 6,3x0,8mm / M6 / 45° (MOQ 1000ks)","100ks",19.743849531083573,{"$f":"F911*(1-Elteq!$F$9)","v":19.743849531083573},"8591735011420"]
["TECHNIK","NDC 28-M3",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 2,8x0,8mm / M3 / 45°","100ks",2.820549933011939,{"$f":"F912*(1-Elteq!$F$9)","v":2.820549933011939},"8591735016043"]
["TECHNIK","NDC 68-M3",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 6,3x0,8mm / M3 / 45°","100ks",4.5277248924665336,{"$f":"F913*(1-Elteq!$F$9)","v":4.5277248924665336},"8591735006693"]
["TECHNIK","NDC 68-M3-90",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 6,3x0,8mm / M3 / 90°","100ks",4.9730748818894712,{"$f":"F914*(1-Elteq!$F$9)","v":4.9730748818894712},"8591735025304"]
["TECHNIK","NDC 68-M4",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 6,3x0,8mm / M4 / 45°","100ks",4.5277248924665336,{"$f":"F915*(1-Elteq!$F$9)","v":4.5277248924665336},"8591735006709"]
["TECHNIK","NDC 68-M4-90",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 6,3x0,8mm / M4 / 90°","100ks",4.9730748818894712,{"$f":"F916*(1-Elteq!$F$9)","v":4.9730748818894712},"8591735025311"]
["TECHNIK","NDC 68-M5",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 6,3x0,8mm / M5 / 45°","100ks",4.5277248924665336,{"$f":"F917*(1-Elteq!$F$9)","v":4.5277248924665336},"8591735006716"]
["TECHNIK","NDC 68-M6",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 6,3x0,8mm / M5 / 45° (MOQ 1000ks)","100ks",23.974674430601482,{"$f":"F918*(1-Elteq!$F$9)","v":23.974674430601482},"8591735006723"]
["TECHNIK","NR 68-M3",null,"Nýtovací plochý kolík mosazný, rozměr 6,3x0,8mm / M3","100ks",2.5607624391818922,{"$f":"F919*(1-Elteq!$F$9)","v":2.5607624391818922},"8591735006730"]
["TECHNIK","NR 68-M4",null,"Nýtovací plochý kolík mosazný, rozměr 6,3x0,8mm / M4","100ks",2.5607624391818922,{"$f":"F920*(1-Elteq!$F$9)","v":2.5607624391818922},"8591735006747"]
["TECHNIK","NR 68-M5",null,"Nýtovací plochý kolík mosazný, rozměr 6,3x0,8mm / M5","100ks",2.5607624391818922,{"$f":"F921*(1-Elteq!$F$9)","v":2.5607624391818922},"8591735006754"]
["TECHNIK","NRC 28-M2",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 2,8x0,8mm / M2","100ks",4.8988498836523151,{"$f":"F922*(1-Elteq!$F$9)","v":4.8988498836523151},"8591735016050"]
["TECHNIK","NRC 48-M3",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 4,8x0,8mm / M3 (MOQ 5000ks)","100ks",3.8968124074507053,{"$f":"F923*(1-Elteq!$F$9)","v":3.8968124074507053},"8591735025328"]
["TECHNIK","NRC 68-M3",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 6,3x0,8mm / M3","100ks",2.8576624321305171,{"$f":"F924*(1-Elteq!$F$9)","v":2.8576624321305171},"8591735006761"]
["TECHNIK","NRC 68-M4",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 6,3x0,8mm / M4","100ks",2.8576624321305171,{"$f":"F925*(1-Elteq!$F$9)","v":2.8576624321305171},"8591735006778"]
["TECHNIK","NRC 68-M5",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 6,3x0,8mm / M5","100ks",2.8576624321305171,{"$f":"F926*(1-Elteq!$F$9)","v":2.8576624321305171},"8591735006785"]
["TECHNIK","NS 68-M3",null,"Nýtovací plochý kolík mosazný 6,3x0,8 / M3","100ks",2.5978749383004702,{"$f":"F927*(1-Elteq!$F$9)","v":2.5978749383004702},"8591735025335"]
["TECHNIK","NS 68-M4",null,"Nýtovací plochý kolík mosazný 6,3x0,8 / M4","100ks",2.5978749383004702,{"$f":"F928*(1-Elteq!$F$9)","v":2.5978749383004702},"8591735012809"]
["TECHNIK","NS 68-M5",null,"Nýtovací plochý kolík mosazný 6,3x0,8 / M5","100ks",2.5978749383004702,{"$f":"F929*(1-Elteq!$F$9)","v":2.5978749383004702},"8591735012793"]
["TECHNIK","NSC 68-M3",null,"Nýtovací plochý kolík mosazný 6,3x0,8 / M3 cínovaný","100ks",3.0432249277234078,{"$f":"F930*(1-Elteq!$F$9)","v":3.0432249277234078},"8591735049232"]
["TECHNIK","NSC 68-M4",null,"Nýtovací plochý kolík mosazný 6,3x0,8 / M4 cínovaný","100ks",3.0432249277234078,{"$f":"F931*(1-Elteq!$F$9)","v":3.0432249277234078},"8591735009540"]
["TECHNIK","NU 45-M3,5",null,"Nýtovací plochý kolík mosazný, rozměr 4,8x0,8mm / M3,5 / 45°","100ks",3.8968124074507053,{"$f":"F932*(1-Elteq!$F$9)","v":3.8968124074507053},""]
["TECHNIK","NU 45-M4",null,"Nýtovací plochý kolík mosazný, rozměr 4,8x0,8mm / M4 / 45°","100ks",3.8968124074507053,{"$f":"F933*(1-Elteq!$F$9)","v":3.8968124074507053},""]
["TECHNIK","NU 45-M5",null,"Nýtovací plochý kolík mosazný, rozměr 4,8x0,8mm / M5 / 45°","100ks",3.8968124074507053,{"$f":"F934*(1-Elteq!$F$9)","v":3.8968124074507053},""]
["TECHNIK","NU 68-M3",null,"Nýtovací plochý kolík mosazný, rozměr 6,3x0,8mm / M3 / 45°","100ks",2.5607624391818922,{"$f":"F935*(1-Elteq!$F$9)","v":2.5607624391818922},"8591735006792"]
["TECHNIK","NU 68-M4",null,"Nýtovací plochý kolík mosazný, rozměr 6,3x0,8mm / M4 / 45°","100ks",2.5607624391818922,{"$f":"F936*(1-Elteq!$F$9)","v":2.5607624391818922},"8591735006808"]
["TECHNIK","NU 68-M4-90",null,"Nýtovací plochý kolík mosazný, rozměr 6,3x0,8mm / M4 / 90°","100ks",3.0432249277234078,{"$f":"F937*(1-Elteq!$F$9)","v":3.0432249277234078},"8591735054052"]
["TECHNIK","NU 68-M5",null,"Nýtovací plochý kolík mosazný, rozměr 6,3x0,8mm / M5 / 45°","100ks",2.5607624391818922,{"$f":"F938*(1-Elteq!$F$9)","v":2.5607624391818922},"8591735006815"]
["TECHNIK","NU 68-M6",null,"Nýtovací plochý kolík mosazný, rozměr 6,3x0,8mm / M6 / 45°","100ks",2.5607624391818922,{"$f":"F939*(1-Elteq!$F$9)","v":2.5607624391818922},"8591735006822"]
["TECHNIK","NUC 28-M3-60",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 2,8x0,8mm / M3 / 60°","100ks",4.00814990480644,{"$f":"F940*(1-Elteq!$F$9)","v":4.00814990480644},"8591735040710"]
["TECHNIK","NUC 28-M3-90",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 2,8x0,8mm / M3 / 90°","100ks",4.00814990480644,{"$f":"F941*(1-Elteq!$F$9)","v":4.00814990480644},"8591735040703"]
["TECHNIK","NUC 45-M3,5",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 4,8x0,5mm / M3,5 / 45°","100ks",4.0823749030435961,{"$f":"F942*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735013547"]
["TECHNIK","NUC 45-M4",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 4,8x0,5mm / M4 / 45°","100ks",4.0823749030435961,{"$f":"F943*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735025342"]
["TECHNIK","NUC 45-M5",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 4,8x0,5mm / M5 / 45°","100ks",4.0823749030435961,{"$f":"F944*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735002510"]
["TECHNIK","NUC 48-M3",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 4,8x0,8mm / M3 / 45°","100ks",2.9689999294862517,{"$f":"F945*(1-Elteq!$F$9)","v":2.9689999294862517},"8591735047092"]
["TECHNIK","NUC 48-M4",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 4,8x0,8mm / M4 / 45°","100ks",2.9689999294862517,{"$f":"F946*(1-Elteq!$F$9)","v":2.9689999294862517},"8591735047085"]
["TECHNIK","NUC 68-M3",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 6,3x0,8mm / M3 / 45°","100ks",2.9318874303676736,{"$f":"F947*(1-Elteq!$F$9)","v":2.9318874303676736},"8591735006839"]
["TECHNIK","NUC 68-M3-90",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 6,3x0,8mm / M3 / 90°","100ks",3.3030124215534551,{"$f":"F948*(1-Elteq!$F$9)","v":3.3030124215534551},"8591735025359"]
["TECHNIK","NUC 68-M4",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 6,3x0,8mm / M4 / 45°","100ks",2.9318874303676736,{"$f":"F949*(1-Elteq!$F$9)","v":2.9318874303676736},"8591735006846"]
["TECHNIK","NUC 68-M4-90",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 6,3x0,8mm / M4 / 90°","100ks",3.3030124215534551,{"$f":"F950*(1-Elteq!$F$9)","v":3.3030124215534551},"8591735025366"]
["TECHNIK","NUC 68-M5",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 6,3x0,8mm / M5 / 45°","100ks",2.9318874303676736,{"$f":"F951*(1-Elteq!$F$9)","v":2.9318874303676736},"8591735006853"]
["TECHNIK","NUC 68-M5-90",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 6,3x0,8mm / M5 / 90°","100ks",3.3030124215534551,{"$f":"F952*(1-Elteq!$F$9)","v":3.3030124215534551},"8591735025373"]
["TECHNIK","NUC 68-M5-90-O",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 6,3x0,8mm / M5 / 90° tvar oka (MOQ 2500ks)","100ks",6.3091248501582848,{"$f":"F953*(1-Elteq!$F$9)","v":6.3091248501582848},""]
["TECHNIK","NUC 68-M6",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 6,3x0,8mm / M6 / 45°","100ks",2.9318874303676736,{"$f":"F954*(1-Elteq!$F$9)","v":2.9318874303676736},"8591735006860"]
["TECHNIK","NUC 68-M8",null,"Nýtovací plochý kolík mosazný cínovaný, rozměr 6,3x0,8mm / M8 / 45° (MOQ 1250ks)","100ks",7.274049827241317,{"$f":"F955*(1-Elteq!$F$9)","v":7.274049827241317},"8591735042349"]
["TECHNIK","NUN 2x68",null,"Nýtovací plochý kolík ocelový niklovaný, rozměr 6,3x0,8mm dvoupólový / úhel 90° (MOQ 1750ks)","100ks",6.4946873457511751,{"$f":"F956*(1-Elteq!$F$9)","v":6.4946873457511751},"8591735054779"]
["TECHNIK","NUN 2x68-M4",null,"Nýtovací plochý kolík ocelový niklovaný, rozměr 6,3x0,8mm dvoupólový / M4 / úhel 45° (MOQ 1250ks)","100ks",8.053412308731458,{"$f":"F957*(1-Elteq!$F$9)","v":8.053412308731458},"8591735054786"]
["TECHNIK","NUN 4x68-M3",null,"Nýtovací plochý kolík ocelový niklovaný, rozměr 6,3x0,8mm čtyřpólový / M3 / úhel 90° (MOQ 500ks)","100ks",9.4265747761188496,{"$f":"F958*(1-Elteq!$F$9)","v":9.4265747761188496},"8591735053871"]
["TECHNIK","NUN 68",null,"Nýtovací plochý kolík ocelový niklovaný, rozměr 6,3x0,8mm / úhel 45°","100ks",4.045262403925018,{"$f":"F959*(1-Elteq!$F$9)","v":4.045262403925018},"8591735019150"]
["TECHNIK","NYT 1x68-45",null,"Nýtovací plochý kolík mosazný, rozměr 6,3x0,8mm/45°/4,0mm jednopólový s trhacím nýtem, uzemňovací","250ks",38.077424095661179,{"$f":"F960*(1-Elteq!$F$9)","v":38.077424095661179},"8591735049553"]
["TECHNIK","NYT 2x68-45",null,"Nýtovací plochý kolík mosazný, rozměr 6,3x0,8mm/45°/4,0mm dvoupólový s trhacím nýtem, uzemňovací","250ks",41.900011504874726,{"$f":"F961*(1-Elteq!$F$9)","v":41.900011504874726},"8591735049560"]
["TECHNIK","NYT 2x68-90",null,"Nýtovací plochý kolík mosazný, rozměr 6,3x0,8mm/90°/3,8mm dvoupólový s trhacím nýtem, uzemňovací","250ks",68.361223376420938,{"$f":"F962*(1-Elteq!$F$9)","v":68.361223376420938},"8591735049591"]
["TECHNIK","NYT 4x68-90",null,"Nýtovací plochý kolík mosazný, rozměr 6,3x0,8mm/90°/3,8mm čtyřpólový s trhacím nýtem, uzemňovací","100ks",72.183810785634492,{"$f":"F963*(1-Elteq!$F$9)","v":72.183810785634492},"8591735049577"]
["TECHNIK","NYTC 1x68-90",null,"Nýtovací plochý kolík cínovaný, rozměr 6,3x0,8mm/90°/4,0mm jednopólový s trhacím nýtem, uzemňovací","250ks",147.70774649194101,{"$f":"F964*(1-Elteq!$F$9)","v":147.70774649194101},"8591735053574"]
["TECHNIK","KRJ 45 bílá",null,"Ochranný pryžový kryt pro konektor RJ 45 bílý","10ks",0.53813123721938316,{"$f":"F965*(1-Elteq!$F$9)","v":0.53813123721938316},"8591735053840"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"KRJ 45 černá",null,"Ochranný pryžový kryt pro konektor RJ 45 černý","10ks",0.53813123721938316,{"$f":"F966*(1-Elteq!$F$9)","v":0.53813123721938316},"8591735019235"]
["TECHNIK","KRJ 45 modrá",null,"Ochranný pryžový kryt pro konektor RJ 45 modrý","10ks",0.53813123721938316,{"$f":"F967*(1-Elteq!$F$9)","v":0.53813123721938316},"8591735019242"]
["TECHNIK","KRJ 45 rudá",null,"Ochranný pryžový kryt pro konektor RJ 45 rudý","10ks",0.53813123721938316,{"$f":"F968*(1-Elteq!$F$9)","v":0.53813123721938316},"8591735019259"]
["TECHNIK","KRJ 45 šedá",null,"Ochranný pryžový kryt pro konektor RJ 45 šedý","10ks",0.53813123721938316,{"$f":"F969*(1-Elteq!$F$9)","v":0.53813123721938316},"8591735019266"]
["TECHNIK","KRJ 45 zelená",null,"Ochranný pryžový kryt pro konektor RJ 45 zelený","10ks",0.53813123721938316,{"$f":"F970*(1-Elteq!$F$9)","v":0.53813123721938316},"8591735019273"]
["TECHNIK","KRJ 45 žlutá",null,"Ochranný pryžový kryt pro konektor RJ 45 žlutý","10ks",0.53813123721938316,{"$f":"F971*(1-Elteq!$F$9)","v":0.53813123721938316},"8591735019280"]
["TECHNIK","KRJ 45V bílá",null,"Ochranný plastový kryt pro konektor RJ 45 bílý","10ks",0.53813123721938316,{"$f":"F972*(1-Elteq!$F$9)","v":0.53813123721938316},"8591735019167"]
["TECHNIK","KRJ 45V černá",null,"Ochranný plastový kryt pro konektor RJ 45 černý","10ks",0.53813123721938316,{"$f":"F973*(1-Elteq!$F$9)","v":0.53813123721938316},"8591735019174"]
["TECHNIK","KRJ 45V modrá",null,"Ochranný plastový kryt pro konektor RJ 45 modrý","10ks",0.53813123721938316,{"$f":"F974*(1-Elteq!$F$9)","v":0.53813123721938316},"8591735019181"]
["TECHNIK","KRJ 45V rudá",null,"Ochranný plastový kryt pro konektor RJ 45 rudý","10ks",0.53813123721938316,{"$f":"F975*(1-Elteq!$F$9)","v":0.53813123721938316},"8591735019198"]
["TECHNIK","KRJ 45V šedá",null,"Ochranný plastový kryt pro konektor RJ 45 šedý","10ks",0.53813123721938316,{"$f":"F976*(1-Elteq!$F$9)","v":0.53813123721938316},"8591735019204"]
["TECHNIK","KRJ 45V zelená",null,"Ochranný plastový kryt pro konektor RJ 45 zelený","10ks",0.53813123721938316,{"$f":"F977*(1-Elteq!$F$9)","v":0.53813123721938316},"8591735019211"]
["TECHNIK","KRJ 45V žlutá",null,"Ochranný plastový kryt pro konektor RJ 45 žlutý","10ks",0.53813123721938316,{"$f":"F978*(1-Elteq!$F$9)","v":0.53813123721938316},"8591735032081"]
["TECHNIK","RJ 10",null,"Konektor RJ10 (4p4c) pro nestíněný neskládaný telefonní kabel typ lanko, CAT.3","100ks",3.265899922434877,{"$f":"F979*(1-Elteq!$F$9)","v":3.265899922434877},"8591735019297"]
["TECHNIK","RJ 11",null,"Konektor RJ11 (6p4c) pro nestíněný neskládaný telefonní kabel typ lanko, CAT.3","100ks",4.0823749030435961,{"$f":"F980*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735019143"]
["TECHNIK","RJ 11-2F",null,"Spojka RJ11 (6p4c) pro konektory RJ11 (2xF)","1ks",0.74224998237156292,{"$f":"F981*(1-Elteq!$F$9)","v":0.74224998237156292},"8591735053802"]
["TECHNIK","RJ 11-2F/M",null,"Rozdvojka RJ11 (6p4c) pro konektory RJ11 (2xF/1xM)","1ks",1.00203747620161,{"$f":"F982*(1-Elteq!$F$9)","v":1.00203747620161},"8591735053833"]
["TECHNIK","RJ 11-3F",null,"Rozdvojka RJ11 (6p4c) pro konektory RJ11 (3xF)","1ks",1.00203747620161,{"$f":"F983*(1-Elteq!$F$9)","v":1.00203747620161},"8591735053796"]
["TECHNIK","RJ 12",null,"Konektor RJ12 (6p6c) pro nestíněný neskládaný telefonní kabel typ lanko, CAT.3","100ks",4.8988498836523151,{"$f":"F984*(1-Elteq!$F$9)","v":4.8988498836523151},"8591735015671"]
["TECHNIK","RJ 45-2F",null,"Spojka RJ45 (8p8c) UTP pro konektory RJ45 (2xF)","1ks",1.00203747620161,{"$f":"F985*(1-Elteq!$F$9)","v":1.00203747620161},"8591735053819"]
["TECHNIK","RJ 45-2F/M",null,"Rozdvojka RJ45 (8p8c) UTP pro konektory RJ45 (2xF/1xM)","1ks",1.9669624532846417,{"$f":"F986*(1-Elteq!$F$9)","v":1.9669624532846417},"8591735053826"]
["TECHNIK","RJ 45-3F",null,"Rozdvojka RJ45 (8p8c) UTP pro konektory RJ45 (3xF)","1ks",1.5958374620988602,{"$f":"F987*(1-Elteq!$F$9)","v":1.5958374620988602},"8591735034306"]
["TECHNIK","RJ 45-D",null,"Konektor RJ45 (8p8c) UTP nestíněný neskládaný pro datový kabel typ drát, CAT.5e","100ks",7.3482748254784731,{"$f":"F988*(1-Elteq!$F$9)","v":7.3482748254784731},"8591735010041"]
["TECHNIK","RJ 45-L",null,"Konektor RJ45 (8p8c) UTP nestíněný neskládaný pro datový kabel typ lanko, CAT.5e","100ks",7.3482748254784731,{"$f":"F989*(1-Elteq!$F$9)","v":7.3482748254784731},"8591735019228"]
["TECHNIK","RJ 45-MDc6",null,"Konektor RJ45 (8p8c) UTP nestíněný skládaný pro datový kabel typ drát, CAT.6","10ks",1.1504874726759224,{"$f":"F990*(1-Elteq!$F$9)","v":1.1504874726759224},"8591735010102"]
["TECHNIK","RJ 45-MDc6v",null,"Konektor RJ45 (8p8c) UTP nestíněný skládaný pro datový kabel typ drát, CAT.6 s vložkou","10ks",1.2247124709130788,{"$f":"F991*(1-Elteq!$F$9)","v":1.2247124709130788},"8591735010058"]
["TECHNIK","RJ 45-MLc6",null,"Konektor RJ45 (8p8c) UTP nestíněný skládaný pro datový kabel typ lanko, CAT.6","10ks",1.1504874726759224,{"$f":"F992*(1-Elteq!$F$9)","v":1.1504874726759224},"8591735003913"]
["TECHNIK","RJ 45-MLc6v",null,"Konektor RJ45 (8p8c) UTP nestíněný skládaný pro datový kabel typ lanko, CAT.6 s vložkou","10ks",1.2247124709130788,{"$f":"F993*(1-Elteq!$F$9)","v":1.2247124709130788},"8591735010782"]
["TECHNIK","RJ 45-S2F",null,"Spojka RJ45 (8p8c) FTP/STP stíněná pro konektory RJ45 (2xF), CAT.5e","1ks",3.6370249136206585,{"$f":"F994*(1-Elteq!$F$9)","v":3.6370249136206585},"8591735038526"]
["TECHNIK","RJ 45-SCLIP",null,"Konektor RJ45 (8p8c) FTP/STP stíněný skládaný s klipem na vodič pro datový kabel s vložkou","10ks",7.7565123157828326,{"$f":"F995*(1-Elteq!$F$9)","v":7.7565123157828326},"8591735053024"]
["TECHNIK","RJ 45-SD",null,"Konektor RJ45 (8p8c) FTP/STP stíněný neskládaný pro datový kabel typ drát, CAT.5e","10ks",1.6329499612174385,{"$f":"F996*(1-Elteq!$F$9)","v":1.6329499612174385},"8591735019303"]
["TECHNIK","RJ 45-SDc6",null,"Konektor RJ45 (8p8c) FTP/STP stíněný skládaný pro datový kabel typ drát, CAT.6","10ks",2.3380874444704234,{"$f":"F997*(1-Elteq!$F$9)","v":2.3380874444704234},"8591735053772"]
["TECHNIK","RJ 45-SDc6v",null,"Konektor RJ45 (8p8c) FTP/STP stíněný skládaný pro datový kabel typ drát, CAT.6 s vložkou","10ks",2.6720999365376263,{"$f":"F998*(1-Elteq!$F$9)","v":2.6720999365376263},"8591735053765"]
["TECHNIK","RJ 45-SL",null,"Konektor RJ45 (8p8c) FTP/STP stíněný neskládaný pro datový kabel typ lanko, CAT.5e","10ks",1.6329499612174385,{"$f":"F999*(1-Elteq!$F$9)","v":1.6329499612174385},"8591735019310"]
["TECHNIK","RJ 45-SLc6",null,"Konektor RJ45 (8p8c) FTP/STP stíněný skládaný pro datový kabel typ lanko, CAT.6","10ks",2.3380874444704234,{"$f":"F1000*(1-Elteq!$F$9)","v":2.3380874444704234},"8591735053789"]
["TECHNIK","RJ 45-SLc6v",null,"Konektor RJ45 (8p8c) FTP/STP stíněný skládaný pro datový kabel typ lanko, CAT.6 s vložkou","10ks",2.6720999365376263,{"$f":"F1001*(1-Elteq!$F$9)","v":2.6720999365376263},"8591735052966"]
["TECHNIK","UB 2A",null,"Spojka zářezová odbočná pro připojení dvou telefonních vodičů o průřezu 0,4-0,9mm2","100ks",26.758111864494843,{"$f":"F1002*(1-Elteq!$F$9)","v":26.758111864494843},""]
["TECHNIK","UR 2",null,"Spojka zářezová pro připojení tří telefonních vodičů o průřezu 0,4-0,9mm2","100ks",18.816037053119121,{"$f":"F1003*(1-Elteq!$F$9)","v":18.816037053119121},"8591735036782"]
["TECHNIK","UY",null,"Spojka zářezová pro připojení dvou telefonních vodičů o průřezu 0,4-0,7mm2","100ks",11.133749735573444,{"$f":"F1004*(1-Elteq!$F$9)","v":11.133749735573444},"8591735026721"]
["TECHNIK","UY 2",null,"Spojka zářezová pro připojení dvou telefonních vodičů o průřezu 0,4-0,9mm2","100ks",11.504874726759224,{"$f":"F1005*(1-Elteq!$F$9)","v":11.504874726759224},"8591735032074"]
["TECHNIK","PKR 68 B",null,"Plochý rozvaděč mosazný 6,3x0,8mm","100ks",10.465724751439037,{"$f":"F1006*(1-Elteq!$F$9)","v":10.465724751439037},"8591735029173"]
["TECHNIK","PKRC 28 B",null,"Plochý rozvaděč mosazný, cínovaný 2,8x0,8mm","100ks",9.4265747761188496,{"$f":"F1007*(1-Elteq!$F$9)","v":9.4265747761188496},"8591735027124"]
["TECHNIK","PKRC 48 B",null,"Plochý rozvaděč mosazný, cínovaný 4,8x0,8mm","100ks",10.577062248794771,{"$f":"F1008*(1-Elteq!$F$9)","v":10.577062248794771},"8591735027070"]
["TECHNIK","PKRC 68 A",null,"Plochý rozvaděč mosazný, cínovaný 6,3x0,8mm","100ks",11.467762227640646,{"$f":"F1009*(1-Elteq!$F$9)","v":11.467762227640646},"8591735016098"]
["TECHNIK","PKRC 68 B",null,"Plochý rozvaděč mosazný, cínovaný 6,3x0,8mm","100ks",15.698587127158556,{"$f":"F1010*(1-Elteq!$F$9)","v":15.698587127158556},"8591735013271"]
["TECHNIK","PKRC 68 C",null,"Plochý rozvaděč mosazný, cínovaný 6,3x0,8mm","100ks",9.5379122734745838,{"$f":"F1011*(1-Elteq!$F$9)","v":9.5379122734745838},"8591735016104"]
["TECHNIK","PKRC 68 D",null,"Plochý rozvaděč mosazný, cínovaný 6,3x0,8mm","100ks",10.799737243506241,{"$f":"F1012*(1-Elteq!$F$9)","v":10.799737243506241},"8591735016111"]
["TECHNIK","PKRC 68 E",null,"Plochý rozvaděč mosazný, cínovaný 6,3x0,8mm","100ks",10.725512245269083,{"$f":"F1013*(1-Elteq!$F$9)","v":10.725512245269083},"8591735016128"]
["TECHNIK","PRI 68/ 2",null,"Plochý rozvaděč izolovaný 6,3x0,8mm PVC, 2-póly (Klauke 800/1)","100ks",14.102749665059696,{"$f":"F1014*(1-Elteq!$F$9)","v":14.102749665059696},"8591735016135"]
["TECHNIK","PRI 68/ 3",null,"Plochý rozvaděč izolovaný 6,3x0,8mm PVC, 3 póly (Klauke 816)","100ks",19.855187028439307,{"$f":"F1015*(1-Elteq!$F$9)","v":19.855187028439307},"8591735016159"]
["TECHNIK","PRI 68/ 4",null,"Plochý rozvaděč izolovaný 6,3x0,8mm PVC, 4 póly (Klauke 800/2)","100ks",33.957936693499001,{"$f":"F1016*(1-Elteq!$F$9)","v":33.957936693499001},"8591735016166"]
["TECHNIK","PRI 68/24",null,"Plochý rozvaděč izolovaný 6,3x0,8mm PVC, 24 pólů (Klauke 800/12)","10ks",21.154124497589542,{"$f":"F1017*(1-Elteq!$F$9)","v":21.154124497589542},"8591735016142"]
["TECHNIK","PRIK 28/ 2",null,"Plochý rozvaděč izolovaný 2,8x0,8mm PVC, 2-póly (Klauke 810/1)","100ks",77.193998166642544,{"$f":"F1018*(1-Elteq!$F$9)","v":77.193998166642544},"8591735029104"]
["TECHNIK","PRIK 28/ 3",null,"Plochý rozvaděč izolovaný 2,8x0,8mm PVC, 3 póly","100ks",65.317998448697537,{"$f":"F1019*(1-Elteq!$F$9)","v":65.317998448697537},""]
["TECHNIK","PRIK 28/ 4",null,"Plochý rozvaděč izolovaný 2,8x0,8mm PVC, 4-póly","50ks",75.709498201899422,{"$f":"F1020*(1-Elteq!$F$9)","v":75.709498201899422},""]
["TECHNIK","PRIK 28/ 6",null,"Plochý rozvaděč izolovaný 2,8x0,8mm PVC, 6 pólů","50ks",62.720123510397066,{"$f":"F1021*(1-Elteq!$F$9)","v":62.720123510397066},""]
["TECHNIK","PRIK 28/24",null,"Plochý rozvaděč izolovaný 2,8x0,8mm PVC, 24-pólů","10ks",88.69887289340177,{"$f":"F1022*(1-Elteq!$F$9)","v":88.69887289340177},""]
["TECHNIK","PRIK 28/36",null,"Plochý rozvaděč izolovaný 2,8x0,8mm PVC, 36 pólů","10ks",70.142623334112699,{"$f":"F1023*(1-Elteq!$F$9)","v":70.142623334112699},""]
["TECHNIK","PRIK 48/ 2",null,"Plochý rozvaděč izolovaný 4,8x0,8mm PVC, 2-póly","100ks",51.21524878363784,{"$f":"F1024*(1-Elteq!$F$9)","v":51.21524878363784},""]
["TECHNIK","PRIK 48/ 4",null,"Plochý rozvaděč izolovaný 4,8x0,8mm PVC, 4-póly","50ks",47.875123862965808,{"$f":"F1025*(1-Elteq!$F$9)","v":47.875123862965808},""]
["TECHNIK","PRIK 48/24",null,"Plochý rozvaděč izolovaný 4,8x0,8mm PVC, 24-pólů","10ks",51.21524878363784,{"$f":"F1026*(1-Elteq!$F$9)","v":51.21524878363784},""]
["TECHNIK","PRIK 68/ 2",null,"Plochý rozvaděč izolovaný 6,3x0,8mm PVC, 2-póly (Klauke 800/1)","100ks",51.21524878363784,{"$f":"F1027*(1-Elteq!$F$9)","v":51.21524878363784},""]
["TECHNIK","PRIK 68/ 4",null,"Plochý rozvaděč izolovaný 6,3x0,8mm PVC, 4-póly (Klauke 800/2)","50ks",47.875123862965808,{"$f":"F1028*(1-Elteq!$F$9)","v":47.875123862965808},""]
["TECHNIK","PRIK 68/24",null,"Plochý rozvaděč izolovaný 6,3x0,8mm PVC, 24-pólů (Klauke 800/12)","10ks",53.44199873075253,{"$f":"F1029*(1-Elteq!$F$9)","v":53.44199873075253},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"KPPS 1,5-25",null,"Kolík plochý se smrštovací bužírkou, průřez 0,5-1,5mm2 / 2,8x0,5mm","100ks",13.842962171229649,{"$f":"F1030*(1-Elteq!$F$9)","v":13.842962171229649},"8591735024840"]
["TECHNIK","KPPS 1,5-28",null,"Kolík plochý se smrštovací bužírkou, průřez 0,5-1,5mm2 / 2,8x0,8mm","100ks",13.842962171229649,{"$f":"F1031*(1-Elteq!$F$9)","v":13.842962171229649},"8591735024505"]
["TECHNIK","KPPS 1,5-45",null,"Kolík plochý se smrštovací bužírkou, průřez 0,5-1,5mm2 / 4,8x0,5mm","100ks",13.842962171229649,{"$f":"F1032*(1-Elteq!$F$9)","v":13.842962171229649},"8591735024857"]
["TECHNIK","KPPS 1,5-48",null,"Kolík plochý se smrštovací bužírkou, průřez 0,5-1,5mm2 / 4,8x0,8mm","100ks",13.842962171229649,{"$f":"F1033*(1-Elteq!$F$9)","v":13.842962171229649},"8591735024512"]
["TECHNIK","KPPS 1,5-68",null,"Kolík plochý se smrštovací bužírkou, průřez 0,5-1,5mm2 / 6,3x0,8mm","100ks",13.842962171229649,{"$f":"F1034*(1-Elteq!$F$9)","v":13.842962171229649},"8591735024529"]
["TECHNIK","KPPS 2,5-45",null,"Kolík plochý se smrštovací bužírkou, průřez 1,5-2,5mm2 / 4,8x0,5mm","100ks",13.842962171229649,{"$f":"F1035*(1-Elteq!$F$9)","v":13.842962171229649},"8591735024864"]
["TECHNIK","KPPS 2,5-48",null,"Kolík plochý se smrštovací bužírkou, průřez 1,5-2,5mm2 / 4,8x0,8mm","100ks",13.842962171229649,{"$f":"F1036*(1-Elteq!$F$9)","v":13.842962171229649},"8591735024871"]
["TECHNIK","KPPS 2,5-68",null,"Kolík plochý se smrštovací bužírkou, průřez 1,5-2,5mm2 / 6,3x0,8mm","100ks",13.842962171229649,{"$f":"F1037*(1-Elteq!$F$9)","v":13.842962171229649},"8591735024536"]
["TECHNIK","KPPS 6-68",null,"Kolík plochý se smrštovací bužírkou, průřez 4-6mm2 / 6,3x0,8mm","100ks",17.925337074273244,{"$f":"F1038*(1-Elteq!$F$9)","v":17.925337074273244},"8591735024543"]
["TECHNIK","OPCS 1,5-68",null,"Objímka plochá se smršťovací bužírkou, průřez 0,5-1,5mm2 / 6,3x0,8mm","100ks",19.298499541660636,{"$f":"F1039*(1-Elteq!$F$9)","v":19.298499541660636},"8591735024550"]
["TECHNIK","OPCS 2,5-68",null,"Objímka plochá se smršťovací bužírkou, průřez 1,5-2,5mm2 / 6,3x0,8mm","100ks",19.669624532846417,{"$f":"F1040*(1-Elteq!$F$9)","v":19.669624532846417},"8591735024819"]
["TECHNIK","OPCS 6-68",null,"Objímka plochá se smršťovací bužírkou, průřez 4-6mm2 / 6,3x0,8mm","100ks",27.277686852154936,{"$f":"F1041*(1-Elteq!$F$9)","v":27.277686852154936},"8591735024826"]
["TECHNIK","OPPS 1,5-25",null,"Objímka plochá se smršťovací bužírkou, průřez 0,5-1,5mm2 / 2,8x0,5mm","100ks",13.360499682688133,{"$f":"F1042*(1-Elteq!$F$9)","v":13.360499682688133},"8591735024802"]
["TECHNIK","OPPS 1,5-28",null,"Objímka plochá se smršťovací bužírkou, průřez 0,5-1,5mm2 / 2,8x0,8mm","100ks",13.360499682688133,{"$f":"F1043*(1-Elteq!$F$9)","v":13.360499682688133},"8591735024567"]
["TECHNIK","OPPS 1,5-45",null,"Objímka plochá se smršťovací bužírkou, průřez 0,5-1,5mm2 / 4,8x0,5mm","100ks",13.360499682688133,{"$f":"F1044*(1-Elteq!$F$9)","v":13.360499682688133},"8591735024833"]
["TECHNIK","OPPS 1,5-48",null,"Objímka plochá se smršťovací bužírkou, průřez 0,5-1,5mm2 / 4,8x0,8mm","100ks",13.360499682688133,{"$f":"F1045*(1-Elteq!$F$9)","v":13.360499682688133},"8591735024574"]
["TECHNIK","OPPS 1,5-68",null,"Objímka plochá se smršťovací bužírkou, průřez 0,5-1,5mm2 / 6,3x0,8mm","100ks",14.102749665059696,{"$f":"F1046*(1-Elteq!$F$9)","v":14.102749665059696},"8591735024581"]
["TECHNIK","OPPS 2,5-25",null,"Objímka plochá se smršťovací bužírkou, průřez 1,5-2,5mm2 / 2,8x0,5mm","100ks",13.360499682688133,{"$f":"F1047*(1-Elteq!$F$9)","v":13.360499682688133},"8591735024888"]
["TECHNIK","OPPS 2,5-28",null,"Objímka plochá se smršťovací bužírkou, průřez 1,5-2,5mm2 / 2,8x0,8mm","100ks",13.360499682688133,{"$f":"F1048*(1-Elteq!$F$9)","v":13.360499682688133},"8591735024895"]
["TECHNIK","OPPS 2,5-45",null,"Objímka plochá se smršťovací bužírkou, průřez 1,5-2,5mm2 / 4,8x0,5mm","100ks",13.360499682688133,{"$f":"F1049*(1-Elteq!$F$9)","v":13.360499682688133},"8591735024901"]
["TECHNIK","OPPS 2,5-48",null,"Objímka plochá se smršťovací bužírkou, průřez 1,5-2,5mm2 / 4,8x0,8mm","100ks",13.360499682688133,{"$f":"F1050*(1-Elteq!$F$9)","v":13.360499682688133},"8591735024918"]
["TECHNIK","OPPS 2,5-68",null,"Objímka plochá se smršťovací bužírkou, průřez 1,5-2,5mm2 / 6,3x0,8mm","100ks",14.102749665059696,{"$f":"F1051*(1-Elteq!$F$9)","v":14.102749665059696},"8591735024598"]
["TECHNIK","OPPS 6-45",null,"Objímka plochá se smršťovací bužírkou, průřez 4-6mm2 / 4,8x0,5mm","100ks",16.886187098953055,{"$f":"F1052*(1-Elteq!$F$9)","v":16.886187098953055},"8591735024925"]
["TECHNIK","OPPS 6-48",null,"Objímka plochá se smršťovací bužírkou, průřez 4-6mm2 / 4,8x0,8mm","100ks",16.886187098953055,{"$f":"F1053*(1-Elteq!$F$9)","v":16.886187098953055},"8591735024932"]
["TECHNIK","OPPS 6-68",null,"Objímka plochá se smršťovací bužírkou, průřez 4-6mm2 / 6,3x0,8mm","100ks",17.44287458573173,{"$f":"F1054*(1-Elteq!$F$9)","v":17.44287458573173},"8591735024604"]
["TECHNIK","KT 28  PA",null,"Kryt objímky jednopólový 2,8mm PA přírodní","100ks",1.8556249559289073,{"$f":"F1055*(1-Elteq!$F$9)","v":1.8556249559289073},"8591735004361"]
["TECHNIK","KT 28 bílá",null,"Kryt objímky jednopólový 2,8mm PE bílá","100ks",1.8185124568103292,{"$f":"F1056*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735006914"]
["TECHNIK","KT 28 černá",null,"Kryt objímky jednopólový 2,8mm PE černá","100ks",1.8185124568103292,{"$f":"F1057*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735006921"]
["TECHNIK","KT 28 modrá",null,"Kryt objímky jednopólový 2,8mm PE modrá","100ks",1.8185124568103292,{"$f":"F1058*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735006945"]
["TECHNIK","KT 28 PVC černá",null,"Kryt objímky jednopólový 2,8mm PVC černá","100ks",5.5668748677867219,{"$f":"F1059*(1-Elteq!$F$9)","v":5.5668748677867219},"8591735029265"]
["TECHNIK","KT 28 PVC modrá",null,"Kryt objímky jednopólový 2,8mm PVC modrá","100ks",5.5668748677867219,{"$f":"F1060*(1-Elteq!$F$9)","v":5.5668748677867219},"8591735033491"]
["TECHNIK","KT 28 PVC rudá",null,"Kryt objímky jednopólový 2,8mm PVC rudá","100ks",5.5668748677867219,{"$f":"F1061*(1-Elteq!$F$9)","v":5.5668748677867219},"8591735029272"]
["TECHNIK","KT 28 PVC transp",null,"Kryt objímky jednopólový 2,8mm PVC transparentní (také v balení 500ks)","100ks",5.1957498766009405,{"$f":"F1062*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735028411"]
["TECHNIK","KT 28 rudá",null,"Kryt objímky jednopólový 2,8mm PE rudá","100ks",1.8185124568103292,{"$f":"F1063*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735006938"]
["TECHNIK","KT 28 žlutá",null,"Kryt objímky jednopólový 2,8mm PE žlutá","100ks",1.8185124568103292,{"$f":"F1064*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735006952"]
["TECHNIK","KT 48  PA",null,"Kryt objímky jednopólový 4,8mm PA přírodní ","100ks",1.8556249559289073,{"$f":"F1065*(1-Elteq!$F$9)","v":1.8556249559289073},"8591735004378"]
["TECHNIK","KT 48  PVC černá",null,"Kryt objímky jednopólový 4,8mm PVC černá","100ks",5.5668748677867219,{"$f":"F1066*(1-Elteq!$F$9)","v":5.5668748677867219},"8591735049881"]
["TECHNIK","KT 48  PVC modrá",null,"Kryt objímky jednopólový 4,8mm PVC modrá","100ks",5.5668748677867219,{"$f":"F1067*(1-Elteq!$F$9)","v":5.5668748677867219},"8591735029968"]
["TECHNIK","KT 48  PVC rudá",null,"Kryt objímky jednopólový 4,8mm PVC rudá","100ks",5.5668748677867219,{"$f":"F1068*(1-Elteq!$F$9)","v":5.5668748677867219},"8591735029951"]
["TECHNIK","KT 48  PVC transp",null,"Kryt objímky jednopólový 4,8mm PVC transparentní (také v balení 500ks)","100ks",5.1957498766009405,{"$f":"F1069*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735021160"]
["TECHNIK","KT 48  PVC žlutá",null,"Kryt objímky jednopólový 4,8mm PVC žlutá","100ks",5.5668748677867219,{"$f":"F1070*(1-Elteq!$F$9)","v":5.5668748677867219},"8591735052775"]
["TECHNIK","KT 48 bílá",null,"Kryt objímky jednopólový 4,8mm PE bílá","100ks",1.8185124568103292,{"$f":"F1071*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735006969"]
["TECHNIK","KT 48 černá",null,"Kryt objímky jednopólový 4,8mm PE černá","100ks",1.8185124568103292,{"$f":"F1072*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735006976"]
["TECHNIK","KT 48 modrá",null,"Kryt objímky jednopólový 4,8mm PE modrá","100ks",1.8185124568103292,{"$f":"F1073*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735011826"]
["TECHNIK","KT 48 rudá",null,"Kryt objímky jednopólový 4,8mm PE rudá","100ks",1.8185124568103292,{"$f":"F1074*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735006983"]
["TECHNIK","KT 48 žlutá",null,"Kryt objímky jednopólový 4,8mm PE žlutá","100ks",1.8185124568103292,{"$f":"F1075*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735007003"]
["TECHNIK","KT 68  PA",null,"Kryt objímky jednopólový 6,3mm PA přírodní ","100ks",1.9298499541660636,{"$f":"F1076*(1-Elteq!$F$9)","v":1.9298499541660636},"8591735004385"]
["TECHNIK","KT 68  PA černá",null,"Kryt objímky jednopólový 6,3mm PA černá","100ks",1.9298499541660636,{"$f":"F1077*(1-Elteq!$F$9)","v":1.9298499541660636},"8591735021924"]
["TECHNIK","KT 68  PVC černá",null,"Kryt objímky jednopólový 6,3mm PVC černá","100ks",5.5668748677867219,{"$f":"F1078*(1-Elteq!$F$9)","v":5.5668748677867219},"8591735021917"]
["TECHNIK","KT 68  PVC modrá",null,"Kryt objímky jednopólový 6,3mm PVC modrá","100ks",5.5668748677867219,{"$f":"F1079*(1-Elteq!$F$9)","v":5.5668748677867219},"8591735021900"]
["TECHNIK","KT 68  PVC rudá",null,"Kryt objímky jednopólový 6,3mm PVC rudá","100ks",5.5668748677867219,{"$f":"F1080*(1-Elteq!$F$9)","v":5.5668748677867219},"8591735021894"]
["TECHNIK","KT 68  PVC transp",null,"Kryt objímky jednopólový 6,3mm PVC transparentní (také v balení 500ks)","100ks",5.1957498766009405,{"$f":"F1081*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735016173"]
["TECHNIK","KT 68  PVC žlutá",null,"Kryt objímky jednopólový 6,3mm PVC žlutá","100ks",5.5668748677867219,{"$f":"F1082*(1-Elteq!$F$9)","v":5.5668748677867219},"8591735021887"]
["TECHNIK","KT 68 bílá",null,"Kryt objímky jednopólový 6,3mm PE bílá","100ks",1.8185124568103292,{"$f":"F1083*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735007010"]
["TECHNIK","KT 68 černá",null,"Kryt objímky jednopólový 6,3mm PE černá","100ks",1.8185124568103292,{"$f":"F1084*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735007027"]
["TECHNIK","KT 68 modrá",null,"Kryt objímky jednopólový 6,3mm PE modrá","100ks",1.8185124568103292,{"$f":"F1085*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735011833"]
["TECHNIK","KT 68 rudá",null,"Kryt objímky jednopólový 6,3mm PE rudá","100ks",1.8185124568103292,{"$f":"F1086*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735007034"]
["TECHNIK","KT 68 žlutá",null,"Kryt objímky jednopólový 6,3mm PE žlutá","100ks",1.8185124568103292,{"$f":"F1087*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735007058"]
["TECHNIK","KTK  1",null,"Kryt kolíku jednopólový PA pro plochý mosazný kolík s jazýčkem 6,3x0,8mm","100ks",6.7915873386998005,{"$f":"F1088*(1-Elteq!$F$9)","v":6.7915873386998005},"8591735007065"]
["TECHNIK","KTK  2",null,"Kryt kolíku dvoupólový PA pro dva ploché mosazné kolíky s jazýčkem 6,3x0,8mm","100ks",8.6472122946287087,{"$f":"F1089*(1-Elteq!$F$9)","v":8.6472122946287087},"8591735007072"]
["TECHNIK","KTK  2T",null,"Kryt kolíku dvoupólový PA pro dva ploché mosazné kolíky s jazýčkem 6,3x0,8mm","100ks",9.6121372717117399,{"$f":"F1090*(1-Elteq!$F$9)","v":9.6121372717117399},"8591735007089"]
["TECHNIK","KTK  3T",null,"Kryt kolíku třípólový PA pro tři ploché mosazné kolíky s jazýčkem 6,3x0,8mm","100ks",9.6121372717117399,{"$f":"F1091*(1-Elteq!$F$9)","v":9.6121372717117399},"8591735007102"]
["TECHNIK","KTK  4",null,"Kryt kolíku čtyřpólový PA pro čtyři ploché mosazné kolíky s jazýčkem 6,3x0,8mm","100ks",15.513024631565665,{"$f":"F1092*(1-Elteq!$F$9)","v":15.513024631565665},"8591735007119"]
["TECHNIK","KTK  6",null,"Kryt kolíku šestipólový PA pro šest plochých mosazných kolíků s jazýčkem 6,3x0,8mm","100ks",13.583174677399601,{"$f":"F1093*(1-Elteq!$F$9)","v":13.583174677399601},"8591735007126"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"KTK  6H",null,"Kryt kolíku šestipólový s háčkem PA pro šest plochých mosazných kolíků s jazýčkem 6,3x0,8mm","100ks",23.974674430601482,{"$f":"F1094*(1-Elteq!$F$9)","v":23.974674430601482},"8591735016180"]
["TECHNIK","KTK  8",null,"Kryt kolíku osmipólový PA pro osm plochých mosazných kolíků s jazýčkem 6,3x0,8mm","100ks",21.376799492301011,{"$f":"F1095*(1-Elteq!$F$9)","v":21.376799492301011},"8591735007133"]
["TECHNIK","KTK 11",null,"Kryt kolíku jedenáctipólový PA pro jedenáct plochých mosazných kolíků s jazýčkem 6,3x0,8mm","100ks",46.761748889408466,{"$f":"F1096*(1-Elteq!$F$9)","v":46.761748889408466},"8591735007140"]
["TECHNIK","KTK 68 bílá",null,"Kryt kolíku jednopólový PE pro plochý mosazný kolík 6,3x0,8mm","100ks",1.7442874585731729,{"$f":"F1097*(1-Elteq!$F$9)","v":1.7442874585731729},"8591735016197"]
["TECHNIK","KTO  1",null,"Kryt objímky jednopólový PA pro plochou mosaznou objímku s jazýčkem 6,3x0,8mm","100ks",5.1215248783637843,{"$f":"F1098*(1-Elteq!$F$9)","v":5.1215248783637843},"8591735007157"]
["TECHNIK","KTO  2",null,"Kryt objímky dvoupólový PA pro dvě ploché mosazné objímky s jazýčkem 6,3x0,8mm","100ks",7.7193998166642546,{"$f":"F1099*(1-Elteq!$F$9)","v":7.7193998166642546},"8591735007164"]
["TECHNIK","KTO  2T",null,"Kryt objímky dvoupólový PA pro dvě ploché mosazné objímky s jazýčkem 6,3x0,8mm","100ks",8.9812247866959112,{"$f":"F1100*(1-Elteq!$F$9)","v":8.9812247866959112},"8591735007171"]
["TECHNIK","KTO  3T",null,"Kryt objímky třípólový PA pro tři ploché mosazné objímky s jazýčkem 6,3x0,8mm","100ks",9.5007997743560058,{"$f":"F1101*(1-Elteq!$F$9)","v":9.5007997743560058},"8591735007195"]
["TECHNIK","KTO  4",null,"Kryt objímky čtyřpólový PA pro čtyři ploché mosazné objímky s jazýčkem 6,3x0,8mm","100ks",16.700624603360165,{"$f":"F1102*(1-Elteq!$F$9)","v":16.700624603360165},"8591735007201"]
["TECHNIK","KTO  6",null,"Kryt objímky šestipólový PA pro šest plochých mosazných objímek s jazýčkem 6,3x0,8mm","100ks",14.362537158889742,{"$f":"F1103*(1-Elteq!$F$9)","v":14.362537158889742},"8591735007218"]
["TECHNIK","KTO  8",null,"Kryt objímky osmipólový PA pro osm plochých mosazných objímek s jazýčkem 6,3x0,8mm","100ks",19.112937046067746,{"$f":"F1104*(1-Elteq!$F$9)","v":19.112937046067746},"8591735007225"]
["TECHNIK","KTO 11",null,"Kryt objímky jedenáctipólový PA pro jedenáct plochých mosazných objímek s jazýčkem 6,3x0,8mm","100ks",46.761748889408466,{"$f":"F1105*(1-Elteq!$F$9)","v":46.761748889408466},"8591735007232"]
["TECHNIK","KTU 28 PA",null,"Kryt objímky úhlový jednopólový 2,8mm PA přírodní","100ks",7.0513748325298478,{"$f":"F1106*(1-Elteq!$F$9)","v":7.0513748325298478},"8591735048426"]
["TECHNIK","KTU 48 PA/2",null,"Kryt objímky úhlový jednopólový 4,8mm PA přírodní","100ks",2.9318874303676736,{"$f":"F1107*(1-Elteq!$F$9)","v":2.9318874303676736},"8591735056070"]
["TECHNIK","KTU 68 PA",null,"Kryt objímky úhlový jednopólový 6,3mm PA přírodní pro objímky s bočním připojením typ A","100ks",3.0432249277234078,{"$f":"F1108*(1-Elteq!$F$9)","v":3.0432249277234078},"8591735007249"]
["TECHNIK","KTU 68 PA/2",null,"Kryt objímky úhlový jednopólový 6,3mm PA přírodní pro objímky s bočním připojením typ B","100ks",2.820549933011939,{"$f":"F1109*(1-Elteq!$F$9)","v":2.820549933011939},"8591735049546"]
["TECHNIK","KTU 68 PVC černá",null,"Kryt objímky úhlový jednopólový 6,3mm PVC černá","100ks",7.0513748325298478,{"$f":"F1110*(1-Elteq!$F$9)","v":7.0513748325298478},"8591735045289"]
["TECHNIK","KTU 68 PVC transp",null,"Kryt objímky úhlový jednopólový 6,3mm PVC transparentní (také v balení 500ks)","100ks",6.6802498413440663,{"$f":"F1111*(1-Elteq!$F$9)","v":6.6802498413440663},"8591735021931"]
["TECHNIK","AL 16-M 8",null,"Oko Al plné dle DIN bez vazelíny, průřez 16mm2 / M8","100ks",56.410998660238782,{"$f":"F1112*(1-Elteq!$F$9)","v":56.410998660238782},"8591735013578"]
["TECHNIK","AL 16-M10",null,"Oko Al plné dle DIN bez vazelíny, průřez 16mm2 / M10","100ks",56.410998660238782,{"$f":"F1113*(1-Elteq!$F$9)","v":56.410998660238782},"8591735013585"]
["TECHNIK","AL 25-M 8",null,"Oko Al plné dle DIN bez vazelíny, průřez 25mm2 / M8","100ks",59.008873598539253,{"$f":"F1114*(1-Elteq!$F$9)","v":59.008873598539253},"8591735013592"]
["TECHNIK","AL 25-M10",null,"Oko Al plné dle DIN bez vazelíny, průřez 25mm2 / M10","100ks",59.008873598539253,{"$f":"F1115*(1-Elteq!$F$9)","v":59.008873598539253},"8591735013608"]
["TECHNIK","AL 25-M12",null,"Oko Al plné dle DIN bez vazelíny, průřez 25mm2 / M12","100ks",59.008873598539253,{"$f":"F1116*(1-Elteq!$F$9)","v":59.008873598539253},"8591735018139"]
["TECHNIK","AL 35-M 8",null,"Oko Al plné dle DIN bez vazelíny, průřez 35mm2 / M8","50ks",32.658999224348769,{"$f":"F1117*(1-Elteq!$F$9)","v":32.658999224348769},"8591735013615"]
["TECHNIK","AL 35-M10",null,"Oko Al plné dle DIN bez vazelíny, průřez 35mm2 / M10","50ks",32.658999224348769,{"$f":"F1118*(1-Elteq!$F$9)","v":32.658999224348769},"8591735012694"]
["TECHNIK","AL 35-M12",null,"Oko Al plné dle DIN bez vazelíny, průřez 35mm2 / M12","50ks",32.658999224348769,{"$f":"F1119*(1-Elteq!$F$9)","v":32.658999224348769},"8591735018146"]
["TECHNIK","AL 50-M 8",null,"Oko Al plné dle DIN bez vazelíny, průřez 50mm2 / M8","50ks",36.741374127392362,{"$f":"F1120*(1-Elteq!$F$9)","v":36.741374127392362},"8591735013356"]
["TECHNIK","AL 50-M10",null,"Oko Al plné dle DIN bez vazelíny, průřez 50mm2 / M10","50ks",36.741374127392362,{"$f":"F1121*(1-Elteq!$F$9)","v":36.741374127392362},"8591735013127"]
["TECHNIK","AL 50-M12",null,"Oko Al plné dle DIN bez vazelíny, průřez 50mm2 / M12","50ks",36.741374127392362,{"$f":"F1122*(1-Elteq!$F$9)","v":36.741374127392362},"8591735013226"]
["TECHNIK","AL 70-M 8",null,"Oko Al plné dle DIN bez vazelíny, průřez 70mm2 / M8","50ks",46.390623898222685,{"$f":"F1123*(1-Elteq!$F$9)","v":46.390623898222685},"8591735020040"]
["TECHNIK","AL 70-M10",null,"Oko Al plné dle DIN bez vazelíny, průřez 70mm2 / M10","50ks",46.390623898222685,{"$f":"F1124*(1-Elteq!$F$9)","v":46.390623898222685},"8591735013622"]
["TECHNIK","AL 70-M12",null,"Oko Al plné dle DIN bez vazelíny, průřez 70mm2 / M12","50ks",46.390623898222685,{"$f":"F1125*(1-Elteq!$F$9)","v":46.390623898222685},"8591735012755"]
["TECHNIK","AL 95-M10",null,"Oko Al plné dle DIN bez vazelíny, průřez 95mm2 / M10","50ks",55.483186182274331,{"$f":"F1126*(1-Elteq!$F$9)","v":55.483186182274331},"8591735013110"]
["TECHNIK","AL 95-M12",null,"Oko Al plné dle DIN bez vazelíny, průřez 95mm2 / M12","50ks",55.483186182274331,{"$f":"F1127*(1-Elteq!$F$9)","v":55.483186182274331},"8591735013639"]
["TECHNIK","AL120-M10",null,"Oko Al plné dle DIN bez vazelíny, průřez 120mm2 / M10","50ks",69.957060838519808,{"$f":"F1128*(1-Elteq!$F$9)","v":69.957060838519808},"8591735013646"]
["TECHNIK","AL120-M12",null,"Oko Al plné dle DIN bez vazelíny, průřez 120mm2 / M12","50ks",69.957060838519808,{"$f":"F1129*(1-Elteq!$F$9)","v":69.957060838519808},"8591735012700"]
["TECHNIK","AL120-M16",null,"Oko Al plné dle DIN bez vazelíny, průřez 120mm2 / M16","50ks",69.957060838519808,{"$f":"F1130*(1-Elteq!$F$9)","v":69.957060838519808},"8591735013653"]
["TECHNIK","AL150-M10",null,"Oko Al plné dle DIN bez vazelíny, průřez 150mm2 / M10","50ks",82.204185547650596,{"$f":"F1131*(1-Elteq!$F$9)","v":82.204185547650596},"8591735013660"]
["TECHNIK","AL150-M12",null,"Oko Al plné dle DIN bez vazelíny, průřez 150mm2 / M12","50ks",82.204185547650596,{"$f":"F1132*(1-Elteq!$F$9)","v":82.204185547650596},"8591735013219"]
["TECHNIK","AL150-M16",null,"Oko Al plné dle DIN bez vazelíny, průřez 150mm2 / M16","50ks",82.204185547650596,{"$f":"F1133*(1-Elteq!$F$9)","v":82.204185547650596},"8591735021337"]
["TECHNIK","AL185-M10",null,"Oko Al plné dle DIN bez vazelíny, průřez 185mm2 / M10","25ks",47.875123862965808,{"$f":"F1134*(1-Elteq!$F$9)","v":47.875123862965808},"8591735013677"]
["TECHNIK","AL185-M12",null,"Oko Al plné dle DIN bez vazelíny, průřez 185mm2 / M12","25ks",46.019498907036898,{"$f":"F1135*(1-Elteq!$F$9)","v":46.019498907036898},"8591735013684"]
["TECHNIK","AL185-M16",null,"Oko Al plné dle DIN bez vazelíny, průřez 185mm2 / M16","25ks",46.019498907036898,{"$f":"F1136*(1-Elteq!$F$9)","v":46.019498907036898},"8591735013691"]
["TECHNIK","AL240-M10",null,"Oko Al plné dle DIN bez vazelíny, průřez 240mm2 / M10","25ks",69.400373351741138,{"$f":"F1137*(1-Elteq!$F$9)","v":69.400373351741138},"8591735013707"]
["TECHNIK","AL240-M12",null,"Oko Al plné dle DIN bez vazelíny, průřez 240mm2 / M12","25ks",69.400373351741138,{"$f":"F1138*(1-Elteq!$F$9)","v":69.400373351741138},"8591735012748"]
["TECHNIK","AL240-M16",null,"Oko Al plné dle DIN bez vazelíny, průřez 240mm2 / M16","25ks",69.400373351741138,{"$f":"F1139*(1-Elteq!$F$9)","v":69.400373351741138},"8591735012649"]
["TECHNIK","AL300-M12",null,"Oko Al plné dle DIN bez vazelíny, průřez 300mm2 / M12","25ks",72.926060768006053,{"$f":"F1140*(1-Elteq!$F$9)","v":72.926060768006053},"8591735019334"]
["TECHNIK","AL300-M16",null,"Oko Al plné dle DIN bez vazelíny, průřez 300mm2 / M16","25ks",72.926060768006053,{"$f":"F1141*(1-Elteq!$F$9)","v":72.926060768006053},"8591735021566"]
["TECHNIK","AL400-M12",null,"Oko Al plné dle DIN bez vazelíny, průřez 400mm2 / M12","10ks",123.02793457808656,{"$f":"F1142*(1-Elteq!$F$9)","v":123.02793457808656},"8591735021573"]
["TECHNIK","AL400-M16",null,"Oko Al plné dle DIN bez vazelíny, průřez 400mm2 / M16","10ks",123.02793457808656,{"$f":"F1143*(1-Elteq!$F$9)","v":123.02793457808656},"8591735021580"]
["TECHNIK","AL500-M12",null,"Oko Al plné dle DIN bez vazelíny, průřez 500mm2 / M12","10ks",132.86274684450976,{"$f":"F1144*(1-Elteq!$F$9)","v":132.86274684450976},"8591735021597"]
["TECHNIK","AL500-M16",null,"Oko Al plné dle DIN bez vazelíny, průřez 500mm2 / M16","10ks",132.86274684450976,{"$f":"F1145*(1-Elteq!$F$9)","v":132.86274684450976},"8591735021603"]
["TECHNIK","AL625-M16",null,"Oko Al plné dle DIN bez vazelíny, průřez 625mm2 / M16","10ks",218.59261980842527,{"$f":"F1146*(1-Elteq!$F$9)","v":218.59261980842527},"8591735041380"]
["TECHNIK","AL-F  16-M 8",null,"Oko Al plné dle DIN s vazelínou, průřez 16mm2 / M8","100ks",113.19312231166334,{"$f":"F1147*(1-Elteq!$F$9)","v":113.19312231166334},"8591735013714"]
["TECHNIK","AL-F  16-M10",null,"Oko Al plné dle DIN s vazelínou, průřez 16mm2 / M10","100ks",113.19312231166334,{"$f":"F1148*(1-Elteq!$F$9)","v":113.19312231166334},"8591735013721"]
["TECHNIK","AL-F  25-M 8",null,"Oko Al plné dle DIN s vazelínou, průřez 25mm2 / M8","100ks",115.04874726759225,{"$f":"F1149*(1-Elteq!$F$9)","v":115.04874726759225},"8591735013738"]
["TECHNIK","AL-F  25-M10",null,"Oko Al plné dle DIN s vazelínou, průřez 25mm2 / M10","100ks",115.04874726759225,{"$f":"F1150*(1-Elteq!$F$9)","v":115.04874726759225},"8591735013745"]
["TECHNIK","AL-F  25-M12",null,"Oko Al plné dle DIN s vazelínou, průřez 25mm2 / M12","100ks",115.04874726759225,{"$f":"F1151*(1-Elteq!$F$9)","v":115.04874726759225},"8591735051068"]
["TECHNIK","AL-F  35-M 8",null,"Oko Al plné dle DIN s vazelínou, průřez 35mm2 / M8","50ks",61.235623545653944,{"$f":"F1152*(1-Elteq!$F$9)","v":61.235623545653944},"8591735013752"]
["TECHNIK","AL-F  35-M10",null,"Oko Al plné dle DIN s vazelínou, průřez 35mm2 / M10","50ks",61.235623545653944,{"$f":"F1153*(1-Elteq!$F$9)","v":61.235623545653944},"8591735012847"]
["TECHNIK","AL-F  35-M12",null,"Oko Al plné dle DIN s vazelínou, průřez 35mm2 / M12","50ks",61.235623545653944,{"$f":"F1154*(1-Elteq!$F$9)","v":61.235623545653944},"8591735051051"]
["TECHNIK","AL-F  50-M 8",null,"Oko Al plné dle DIN s vazelínou, průřez 50mm2 / M8","50ks",52.88531124397386,{"$f":"F1155*(1-Elteq!$F$9)","v":52.88531124397386},"8591735013769"]
["TECHNIK","AL-F  50-M10",null,"Oko Al plné dle DIN s vazelínou, průřez 50mm2 / M10","50ks",52.88531124397386,{"$f":"F1156*(1-Elteq!$F$9)","v":52.88531124397386},"8591735012687"]
["TECHNIK","AL-F  50-M12",null,"Oko Al plné dle DIN s vazelínou, průřez 50mm2 / M12","50ks",52.88531124397386,{"$f":"F1157*(1-Elteq!$F$9)","v":52.88531124397386},"8591735013776"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"AL-F  70-M 8",null,"Oko Al plné dle DIN s vazelínou, průřez 70mm2 / M8","50ks",62.905686005989956,{"$f":"F1158*(1-Elteq!$F$9)","v":62.905686005989956},"8591735045494"]
["TECHNIK","AL-F  70-M10",null,"Oko Al plné dle DIN s vazelínou, průřez 70mm2 / M10","50ks",62.905686005989956,{"$f":"F1159*(1-Elteq!$F$9)","v":62.905686005989956},"8591735012717"]
["TECHNIK","AL-F  70-M12",null,"Oko Al plné dle DIN s vazelínou, průřez 70mm2 / M12","50ks",62.905686005989956,{"$f":"F1160*(1-Elteq!$F$9)","v":62.905686005989956},"8591735012830"]
["TECHNIK","AL-F  70-M16",null,"Oko Al plné dle DIN s vazelínou, průřez 70mm2 / M16","50ks",72.926060768006053,{"$f":"F1161*(1-Elteq!$F$9)","v":72.926060768006053},"8591735019044"]
["TECHNIK","AL-F  95-M10",null,"Oko Al plné dle DIN s vazelínou, průřez 95mm2 / M10","50ks",79.049623122571447,{"$f":"F1162*(1-Elteq!$F$9)","v":79.049623122571447},"8591735013783"]
["TECHNIK","AL-F  95-M12",null,"Oko Al plné dle DIN s vazelínou, průřez 95mm2 / M12","50ks",79.049623122571447,{"$f":"F1163*(1-Elteq!$F$9)","v":79.049623122571447},"8591735013790"]
["TECHNIK","AL-F  95-M16",null,"Oko Al plné dle DIN s vazelínou, průřez 95mm2 / M16","50ks",79.049623122571447,{"$f":"F1164*(1-Elteq!$F$9)","v":79.049623122571447},"8591735027162"]
["TECHNIK","AL-F 120-M10",null,"Oko Al plné dle DIN s vazelínou, průřez 120mm2 / M10","50ks",79.049623122571447,{"$f":"F1165*(1-Elteq!$F$9)","v":79.049623122571447},"8591735013806"]
["TECHNIK","AL-F 120-M12",null,"Oko Al plné dle DIN s vazelínou, průřez 120mm2 / M12","50ks",79.049623122571447,{"$f":"F1166*(1-Elteq!$F$9)","v":79.049623122571447},"8591735012724"]
["TECHNIK","AL-F 120-M16",null,"Oko Al plné dle DIN s vazelínou, průřez 120mm2 / M16","50ks",79.049623122571447,{"$f":"F1167*(1-Elteq!$F$9)","v":79.049623122571447},"8591735008895"]
["TECHNIK","AL-F 150-M10",null,"Oko Al plné dle DIN s vazelínou, průřez 150mm2 / M10","50ks",101.31712259371834,{"$f":"F1168*(1-Elteq!$F$9)","v":101.31712259371834},"8591735013448"]
["TECHNIK","AL-F 150-M12",null,"Oko Al plné dle DIN s vazelínou, průřez 150mm2 / M12","50ks",101.31712259371834,{"$f":"F1169*(1-Elteq!$F$9)","v":101.31712259371834},"8591735013813"]
["TECHNIK","AL-F 150-M16",null,"Oko Al plné dle DIN s vazelínou, průřez 150mm2 / M16","50ks",101.31712259371834,{"$f":"F1170*(1-Elteq!$F$9)","v":101.31712259371834},"8591735019051"]
["TECHNIK","AL-F 185-M10",null,"Oko Al plné dle DIN s vazelínou, průřez 185mm2 / M10","25ks",66.98806090903355,{"$f":"F1171*(1-Elteq!$F$9)","v":66.98806090903355},"8591735013820"]
["TECHNIK","AL-F 185-M12",null,"Oko Al plné dle DIN s vazelínou, průřez 185mm2 / M12","25ks",65.78190468767977,{"$f":"F1172*(1-Elteq!$F$9)","v":65.78190468767977},"8591735013837"]
["TECHNIK","AL-F 185-M16",null,"Oko Al plné dle DIN s vazelínou, průřez 185mm2 / M16","25ks",65.78190468767977,{"$f":"F1173*(1-Elteq!$F$9)","v":65.78190468767977},"8591735013844"]
["TECHNIK","AL-F 240-M10",null,"Oko Al plné dle DIN s vazelínou, průřez 240mm2 / M10","25ks",86.843247937472867,{"$f":"F1174*(1-Elteq!$F$9)","v":86.843247937472867},"8591735013103"]
["TECHNIK","AL-F 240-M12",null,"Oko Al plné dle DIN s vazelínou, průřez 240mm2 / M12","25ks",85.637091716119073,{"$f":"F1175*(1-Elteq!$F$9)","v":85.637091716119073},"8591735013097"]
["TECHNIK","AL-F 240-M16",null,"Oko Al plné dle DIN s vazelínou, průřez 240mm2 / M16","25ks",85.637091716119073,{"$f":"F1176*(1-Elteq!$F$9)","v":85.637091716119073},"8591735012823"]
["TECHNIK","AL-F 300-M12",null,"Oko Al plné dle DIN s vazelínou, průřez 300mm2 / M12","25ks",97.69865392965697,{"$f":"F1177*(1-Elteq!$F$9)","v":97.69865392965697},"8591735020897"]
["TECHNIK","AL-F 300-M16",null,"Oko Al plné dle DIN s vazelínou, průřez 300mm2 / M16","25ks",97.69865392965697,{"$f":"F1178*(1-Elteq!$F$9)","v":97.69865392965697},"8591735020903"]
["TECHNIK","AL-F 400-M12",null,"Oko Al plné dle DIN s vazelínou, průřez 400mm2 / M12","10ks",126.40517199787716,{"$f":"F1179*(1-Elteq!$F$9)","v":126.40517199787716},"8591735050979"]
["TECHNIK","AL-F 400-M16",null,"Oko Al plné dle DIN s vazelínou, průřez 400mm2 / M16","10ks",126.40517199787716,{"$f":"F1180*(1-Elteq!$F$9)","v":126.40517199787716},"8591735042035"]
["TECHNIK","AL-F 500-M12",null,"Oko Al plné dle DIN s vazelínou, průřez 500mm2 / M12","10ks",143.77382158537173,{"$f":"F1181*(1-Elteq!$F$9)","v":143.77382158537173},"8591735015879"]
["TECHNIK","AL-F 500-M16",null,"Oko Al plné dle DIN s vazelínou, průřez 500mm2 / M16","10ks",143.77382158537173,{"$f":"F1182*(1-Elteq!$F$9)","v":143.77382158537173},"8591735017804"]
["TECHNIK","AL-F 625-M16",null,"Oko Al plné dle DIN s vazelínou, průřez 625mm2 / M16","10ks",301.05659284990594,{"$f":"F1183*(1-Elteq!$F$9)","v":301.05659284990594},"8591735041397"]
["TECHNIK","KUV   6-M 5",null,"Oko Cu dle DIN 46235 cínované, průřez 6mm2 / M5","100ks",42.679373986364865,{"$f":"F1184*(1-Elteq!$F$9)","v":42.679373986364865},"8591735028763"]
["TECHNIK","KUV   6-M 6",null,"Oko Cu dle DIN 46235 cínované, průřez 6mm2 / M6","100ks",42.679373986364865,{"$f":"F1185*(1-Elteq!$F$9)","v":42.679373986364865},"8591735028770"]
["TECHNIK","KUV   6-M 8",null,"Oko Cu dle DIN 46235 cínované, průřez 6mm2 / M8","100ks",74.224998237156285,{"$f":"F1186*(1-Elteq!$F$9)","v":74.224998237156285},"8591735028787"]
["TECHNIK","KUV  10-M 4",null,"Oko Cu dle DIN 46235 cínované, průřez 10mm2 / M4","100ks",79.420748113757227,{"$f":"F1187*(1-Elteq!$F$9)","v":79.420748113757227},"8591735028794"]
["TECHNIK","KUV  10-M 5",null,"Oko Cu dle DIN 46235 cínované, průřez 10mm2 / M5","100ks",42.679373986364865,{"$f":"F1188*(1-Elteq!$F$9)","v":42.679373986364865},"8591735020361"]
["TECHNIK","KUV  10-M 6",null,"Oko Cu dle DIN 46235 cínované, průřez 10mm2 / M6","100ks",42.679373986364865,{"$f":"F1189*(1-Elteq!$F$9)","v":42.679373986364865},"8591735028800"]
["TECHNIK","KUV  10-M 8",null,"Oko Cu dle DIN 46235 cínované, průřez 10mm2 / M8","100ks",51.957498766009401,{"$f":"F1190*(1-Elteq!$F$9)","v":51.957498766009401},"8591735028817"]
["TECHNIK","KUV  10-M10",null,"Oko Cu dle DIN 46235 cínované, průřez 10mm2 / M10","100ks",69.400373351741138,{"$f":"F1191*(1-Elteq!$F$9)","v":69.400373351741138},"8591735028824"]
["TECHNIK","KUV  16-M 6",null,"Oko Cu dle DIN 46235 cínované, průřez 16mm2 / M6","100ks",63.462373492768627,{"$f":"F1192*(1-Elteq!$F$9)","v":63.462373492768627},"8591735031411"]
["TECHNIK","KUV  16-M 8",null,"Oko Cu dle DIN 46235 cínované, průřez 16mm2 / M8","100ks",61.977873528025505,{"$f":"F1193*(1-Elteq!$F$9)","v":61.977873528025505},"8591735028831"]
["TECHNIK","KUV  16-M10",null,"Oko Cu dle DIN 46235 cínované, průřez 16mm2 / M10","100ks",61.977873528025505,{"$f":"F1194*(1-Elteq!$F$9)","v":61.977873528025505},"8591735031589"]
["TECHNIK","KUV  16-M12",null,"Oko Cu dle DIN 46235 cínované, průřez 16mm2 / M12","100ks",64.204623475140195,{"$f":"F1195*(1-Elteq!$F$9)","v":64.204623475140195},"8591735031596"]
["TECHNIK","KUV  25-M 6",null,"Oko Cu dle DIN 46235 cínované, průřez 25mm2 / M6","50ks",43.050498977550646,{"$f":"F1196*(1-Elteq!$F$9)","v":43.050498977550646},"8591735031640"]
["TECHNIK","KUV  25-M 8",null,"Oko Cu dle DIN 46235 cínované, průřez 25mm2 / M8","100ks",80.534123087314583,{"$f":"F1197*(1-Elteq!$F$9)","v":80.534123087314583},"8591735028848"]
["TECHNIK","KUV  25-M10",null,"Oko Cu dle DIN 46235 cínované, průřez 25mm2 / M10","100ks",80.534123087314583,{"$f":"F1198*(1-Elteq!$F$9)","v":80.534123087314583},"8591735028855"]
["TECHNIK","KUV  25-M12",null,"Oko Cu dle DIN 46235 cínované, průřez 25mm2 / M12","25ks",20.782999506403762,{"$f":"F1199*(1-Elteq!$F$9)","v":20.782999506403762},"8591735031657"]
["TECHNIK","KUV  35-M 6",null,"Oko Cu dle DIN 46235 cínované, průřez 35mm2 / M6","25ks",27.556030595544275,{"$f":"F1200*(1-Elteq!$F$9)","v":27.556030595544275},"8591735031664"]
["TECHNIK","KUV  35-M 8",null,"Oko Cu dle DIN 46235 cínované, průřez 35mm2 / M8","50ks",55.11206119108855,{"$f":"F1201*(1-Elteq!$F$9)","v":55.11206119108855},"8591735028862"]
["TECHNIK","KUV  35-M10",null,"Oko Cu dle DIN 46235 cínované, průřez 35mm2 / M10","50ks",55.11206119108855,{"$f":"F1202*(1-Elteq!$F$9)","v":55.11206119108855},"8591735028879"]
["TECHNIK","KUV  35-M12",null,"Oko Cu dle DIN 46235 cínované, průřez 35mm2 / M12","50ks",55.668748677867221,{"$f":"F1203*(1-Elteq!$F$9)","v":55.668748677867221},"8591735028886"]
["TECHNIK","KUV  35-M16",null,"Oko Cu dle DIN 46235 cínované, průřez 35mm2 / M16","50ks",62.348998519211285,{"$f":"F1204*(1-Elteq!$F$9)","v":62.348998519211285},"8591735031671"]
["TECHNIK","KUV  50-M 6",null,"Oko Cu dle DIN 46235 cínované, průřez 50mm2 / M6","50ks",84.98762298154395,{"$f":"F1205*(1-Elteq!$F$9)","v":84.98762298154395},"8591735031688"]
["TECHNIK","KUV  50-M 8",null,"Oko Cu dle DIN 46235 cínované, průřez 50mm2 / M8","50ks",84.98762298154395,{"$f":"F1206*(1-Elteq!$F$9)","v":84.98762298154395},"8591735028893"]
["TECHNIK","KUV  50-M10",null,"Oko Cu dle DIN 46235 cínované, průřez 50mm2 / M10","50ks",85.358747972729731,{"$f":"F1207*(1-Elteq!$F$9)","v":85.358747972729731},"8591735028909"]
["TECHNIK","KUV  50-M12",null,"Oko Cu dle DIN 46235 cínované, průřez 50mm2 / M12","50ks",85.358747972729731,{"$f":"F1208*(1-Elteq!$F$9)","v":85.358747972729731},"8591735028916"]
["TECHNIK","KUV  50-M16",null,"Oko Cu dle DIN 46235 cínované, průřez 50mm2 / M16","50ks",93.152372787631151,{"$f":"F1209*(1-Elteq!$F$9)","v":93.152372787631151},"8591735031695"]
["TECHNIK","KUV  70-M 8",null,"Oko Cu dle DIN 46235 cínované, průřez 70mm2 / M8","50ks",112.26530983369889,{"$f":"F1210*(1-Elteq!$F$9)","v":112.26530983369889},"8591735028923"]
["TECHNIK","KUV  70-M10",null,"Oko Cu dle DIN 46235 cínované, průřez 70mm2 / M10","50ks",112.26530983369889,{"$f":"F1211*(1-Elteq!$F$9)","v":112.26530983369889},"8591735028930"]
["TECHNIK","KUV  70-M12",null,"Oko Cu dle DIN 46235 cínované, průřez 70mm2 / M12","50ks",113.19312231166334,{"$f":"F1212*(1-Elteq!$F$9)","v":113.19312231166334},"8591735028947"]
["TECHNIK","KUV  70-M16",null,"Oko Cu dle DIN 46235 cínované, průřez 70mm2 / M16","25ks",69.400373351741138,{"$f":"F1213*(1-Elteq!$F$9)","v":69.400373351741138},"8591735031701"]
["TECHNIK","KUV  70-M20",null,"Oko Cu dle DIN 46235 cínované, průřez 70mm2 / M20","25ks",83.688685512393718,{"$f":"F1214*(1-Elteq!$F$9)","v":83.688685512393718},"8591735054120"]
["TECHNIK","KUV  95-M 8",null,"Oko Cu dle DIN 46235 cínované, průřez 95mm2 / M8","50ks",150.67674642142728,{"$f":"F1215*(1-Elteq!$F$9)","v":150.67674642142728},"8591735031718"]
["TECHNIK","KUV  95-M10",null,"Oko Cu dle DIN 46235 cínované, průřez 95mm2 / M10","50ks",150.67674642142728,{"$f":"F1216*(1-Elteq!$F$9)","v":150.67674642142728},"8591735028954"]
["TECHNIK","KUV  95-M12",null,"Oko Cu dle DIN 46235 cínované, průřez 95mm2 / M12","50ks",152.1612463861704,{"$f":"F1217*(1-Elteq!$F$9)","v":152.1612463861704},"8591735028961"]
["TECHNIK","KUV  95-M16",null,"Oko Cu dle DIN 46235 cínované, průřez 95mm2 / M16","50ks",161.06824617462917,{"$f":"F1218*(1-Elteq!$F$9)","v":161.06824617462917},"8591735028978"]
["TECHNIK","KUV 120-M10",null,"Oko Cu dle DIN 46235 cínované, průřez 120mm2 / M10","50ks",181.85124568103291,{"$f":"F1219*(1-Elteq!$F$9)","v":181.85124568103291},"8591735028985"]
["TECHNIK","KUV 120-M12",null,"Oko Cu dle DIN 46235 cínované, průřez 120mm2 / M12","50ks",181.85124568103291,{"$f":"F1220*(1-Elteq!$F$9)","v":181.85124568103291},"8591735028992"]
["TECHNIK","KUV 120-M16",null,"Oko Cu dle DIN 46235 cínované, průřez 120mm2 / M16","50ks",189.27374550474855,{"$f":"F1221*(1-Elteq!$F$9)","v":189.27374550474855},"8591735029005"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"KUV 120-M20",null,"Oko Cu dle DIN 46235 cínované, průřez 120mm2 / M20","50ks",195.9539953460926,{"$f":"F1222*(1-Elteq!$F$9)","v":195.9539953460926},"8591735031602"]
["TECHNIK","KUV 150-M10",null,"Oko Cu dle DIN 46235 cínované, průřez 150mm2 / M10","10ks",50.844123792452059,{"$f":"F1223*(1-Elteq!$F$9)","v":50.844123792452059},"8591735031619"]
["TECHNIK","KUV 150-M12",null,"Oko Cu dle DIN 46235 cínované, průřez 150mm2 / M12","25ks",127.11030948113014,{"$f":"F1224*(1-Elteq!$F$9)","v":127.11030948113014},"8591735031725"]
["TECHNIK","KUV 150-M16",null,"Oko Cu dle DIN 46235 cínované, průřez 150mm2 / M16","10ks",51.957498766009401,{"$f":"F1225*(1-Elteq!$F$9)","v":51.957498766009401},"8591735031732"]
["TECHNIK","KUV 150-M20",null,"Oko Cu dle DIN 46235 cínované, průřez 150mm2 / M20","10ks",57.895498624981904,{"$f":"F1226*(1-Elteq!$F$9)","v":57.895498624981904},"8591735031749"]
["TECHNIK","KUV 185-M10",null,"Oko Cu dle DIN 46235 cínované, průřez 185mm2 / M10","10ks",54.184248713124092,{"$f":"F1227*(1-Elteq!$F$9)","v":54.184248713124092},"8591735031756"]
["TECHNIK","KUV 185-M12",null,"Oko Cu dle DIN 46235 cínované, průřez 185mm2 / M12","10ks",54.184248713124092,{"$f":"F1228*(1-Elteq!$F$9)","v":54.184248713124092},"8591735031626"]
["TECHNIK","KUV 185-M16",null,"Oko Cu dle DIN 46235 cínované, průřez 185mm2 / M16","25ks",135.46062178281022,{"$f":"F1229*(1-Elteq!$F$9)","v":135.46062178281022},"8591735031763"]
["TECHNIK","KUV 185-M20",null,"Oko Cu dle DIN 46235 cínované, průřez 185mm2 / M20","25ks",163.29499612174385,{"$f":"F1230*(1-Elteq!$F$9)","v":163.29499612174385},"8591735031770"]
["TECHNIK","KUV 240-M10",null,"Oko Cu dle DIN 46235 cínované, průřez 240mm2 / M10","10ks",85.729872963915511,{"$f":"F1231*(1-Elteq!$F$9)","v":85.729872963915511},"8591735031787"]
["TECHNIK","KUV 240-M12",null,"Oko Cu dle DIN 46235 cínované, průřez 240mm2 / M12","10ks",85.729872963915511,{"$f":"F1232*(1-Elteq!$F$9)","v":85.729872963915511},"8591735029395"]
["TECHNIK","KUV 240-M16",null,"Oko Cu dle DIN 46235 cínované, průřez 240mm2 / M16","25ks",215.25249488775324,{"$f":"F1233*(1-Elteq!$F$9)","v":215.25249488775324},"8591735029012"]
["TECHNIK","KUV 240-M20",null,"Oko Cu dle DIN 46235 cínované, průřez 240mm2 / M20","25ks",222.67499471146888,{"$f":"F1234*(1-Elteq!$F$9)","v":222.67499471146888},"8591735029029"]
["TECHNIK","KUV 300-M12",null,"Oko Cu dle DIN 46235 cínované, průřez 300mm2 / M12","5ks",47.132873880594246,{"$f":"F1235*(1-Elteq!$F$9)","v":47.132873880594246},"8591735029494"]
["TECHNIK","KUV 300-M16",null,"Oko Cu dle DIN 46235 cínované, průřez 300mm2 / M16","5ks",47.132873880594246,{"$f":"F1236*(1-Elteq!$F$9)","v":47.132873880594246},"8591735029982"]
["TECHNIK","KUV 300-M20",null,"Oko Cu dle DIN 46235 cínované, průřez 300mm2 / M20","5ks",47.503998871780027,{"$f":"F1237*(1-Elteq!$F$9)","v":47.503998871780027},"8591735031794"]
["TECHNIK","KUV 400-M16",null,"Oko Cu dle DIN 46235 cínované, průřez 400mm2 / M16","20ks",359.24899146783645,{"$f":"F1238*(1-Elteq!$F$9)","v":359.24899146783645},"8591735031633"]
["TECHNIK","KUV 400-M20",null,"Oko Cu dle DIN 46235 cínované, průřez 400mm2 / M20","20ks",359.24899146783645,{"$f":"F1239*(1-Elteq!$F$9)","v":359.24899146783645},"8591735031800"]
["TECHNIK","KUV 500-2xM16/40",null,"Oko Cu dle DIN 46235 cínované, průřez 500mm2 / 2xM16, rozteč 40mm","1ks",35.25687416264924,{"$f":"F1240*(1-Elteq!$F$9)","v":35.25687416264924},""]
["TECHNIK","KUV 500-M12",null,"Oko Cu dle DIN 46235 cínované, průřez 500mm2 / M12","20ks",516.60598773060781,{"$f":"F1241*(1-Elteq!$F$9)","v":516.60598773060781},"8591735037260"]
["TECHNIK","KUV 500-M16",null,"Oko Cu dle DIN 46235 cínované, průřez 500mm2 / M16","20ks",516.60598773060781,{"$f":"F1242*(1-Elteq!$F$9)","v":516.60598773060781},"8591735031817"]
["TECHNIK","KUV 500-M20",null,"Oko Cu dle DIN 46235 cínované, průřez 500mm2 / M20","20ks",516.60598773060781,{"$f":"F1243*(1-Elteq!$F$9)","v":516.60598773060781},"8591735031824"]
["TECHNIK","KUV 625-M16",null,"Oko Cu dle DIN 46235 cínované, průřez 625mm2 / M16","1ks",28.465286823949437,{"$f":"F1244*(1-Elteq!$F$9)","v":28.465286823949437},""]
["TECHNIK","OL  0,75-M 3",null,"Oko lehčené Cu pocínované, průřez 0,75mm2 / M3","100ks",17.81399957691751,{"$f":"F1245*(1-Elteq!$F$9)","v":17.81399957691751},"8591735022389"]
["TECHNIK","OL  0,75-M 4",null,"Oko lehčené Cu pocínované, průřez 0,75mm2 / M4","100ks",17.81399957691751,{"$f":"F1246*(1-Elteq!$F$9)","v":17.81399957691751},"8591735022396"]
["TECHNIK","OL  0,75-M 5",null,"Oko lehčené Cu pocínované, průřez 0,75mm2 / M5","100ks",20.040749524032197,{"$f":"F1247*(1-Elteq!$F$9)","v":20.040749524032197},"8591735022402"]
["TECHNIK","OL  1,5-M 3",null,"Oko lehčené Cu pocínované, průřez 1,5mm2 / M3","100ks",20.782999506403762,{"$f":"F1248*(1-Elteq!$F$9)","v":20.782999506403762},"8591735002930"]
["TECHNIK","OL  1,5-M 4",null,"Oko lehčené Cu pocínované, průřez 1,5mm2 / M4","100ks",20.782999506403762,{"$f":"F1249*(1-Elteq!$F$9)","v":20.782999506403762},"8591735002947"]
["TECHNIK","OL  1,5-M 5",null,"Oko lehčené Cu pocínované, průřez 1,5mm2 / M5","100ks",21.154124497589542,{"$f":"F1250*(1-Elteq!$F$9)","v":21.154124497589542},"8591735002954"]
["TECHNIK","OL  1,5-M 6",null,"Oko lehčené Cu pocínované, průřez 1,5mm2 / M6","100ks",21.154124497589542,{"$f":"F1251*(1-Elteq!$F$9)","v":21.154124497589542},"8591735002961"]
["TECHNIK","OL  2,5-M 3",null,"Oko lehčené Cu pocínované, průřez 2,5mm2 / M3","100ks",21.525249488775323,{"$f":"F1252*(1-Elteq!$F$9)","v":21.525249488775323},"8591735014322"]
["TECHNIK","OL  2,5-M 4",null,"Oko lehčené Cu pocínované, průřez 2,5mm2 / M4","100ks",21.525249488775323,{"$f":"F1253*(1-Elteq!$F$9)","v":21.525249488775323},"8591735002985"]
["TECHNIK","OL  2,5-M 5",null,"Oko lehčené Cu pocínované, průřez 2,5mm2 / M5","100ks",21.525249488775323,{"$f":"F1254*(1-Elteq!$F$9)","v":21.525249488775323},"8591735002992"]
["TECHNIK","OL  2,5-M 6",null,"Oko lehčené Cu pocínované, průřez 2,5mm2 / M6","100ks",21.525249488775323,{"$f":"F1255*(1-Elteq!$F$9)","v":21.525249488775323},"8591735003005"]
["TECHNIK","OL  2,5-M 8",null,"Oko lehčené Cu pocínované, průřez 2,5mm2 / M8","100ks",27.092124356562046,{"$f":"F1256*(1-Elteq!$F$9)","v":27.092124356562046},"8591735002978"]
["TECHNIK","OL  4-M 4",null,"Oko lehčené Cu pocínované, průřez 4mm2 / M4","100ks",24.123124427075794,{"$f":"F1257*(1-Elteq!$F$9)","v":24.123124427075794},"8591735003012"]
["TECHNIK","OL  4-M 5",null,"Oko lehčené Cu pocínované, průřez 4mm2 / M5","100ks",24.494249418261575,{"$f":"F1258*(1-Elteq!$F$9)","v":24.494249418261575},"8591735003029"]
["TECHNIK","OL  4-M 6",null,"Oko lehčené Cu pocínované, průřez 4mm2 / M6","100ks",24.494249418261575,{"$f":"F1259*(1-Elteq!$F$9)","v":24.494249418261575},"8591735003036"]
["TECHNIK","OL  4-M 8",null,"Oko lehčené Cu pocínované, průřez 4mm2 / M8","100ks",26.349874374190485,{"$f":"F1260*(1-Elteq!$F$9)","v":26.349874374190485},"8591735003043"]
["TECHNIK","OL  4-M10 ",null,"Oko lehčené Cu pocínované, průřez 4mm2 / M10","100ks",31.174499259605643,{"$f":"F1261*(1-Elteq!$F$9)","v":31.174499259605643},"8591735035303"]
["TECHNIK","OL  6-M 4",null,"Oko lehčené Cu pocínované, průřez 6mm2 / M4","100ks",24.865374409447359,{"$f":"F1262*(1-Elteq!$F$9)","v":24.865374409447359},"8591735021528"]
["TECHNIK","OL  6-M 5",null,"Oko lehčené Cu pocínované, průřez 6mm2 / M5","100ks",24.494249418261575,{"$f":"F1263*(1-Elteq!$F$9)","v":24.494249418261575},"8591735003050"]
["TECHNIK","OL  6-M 6",null,"Oko lehčené Cu pocínované, průřez 6mm2 / M6","100ks",24.494249418261575,{"$f":"F1264*(1-Elteq!$F$9)","v":24.494249418261575},"8591735003067"]
["TECHNIK","OL  6-M 8",null,"Oko lehčené Cu pocínované, průřez 6mm2 / M8","100ks",24.865374409447359,{"$f":"F1265*(1-Elteq!$F$9)","v":24.865374409447359},"8591735003074"]
["TECHNIK","OL  6-M10",null,"Oko lehčené Cu pocínované, průřez 6mm2 / M10","100ks",30.803374268419862,{"$f":"F1266*(1-Elteq!$F$9)","v":30.803374268419862},"8591735003081"]
["TECHNIK","OL  6-M12",null,"Oko lehčené Cu pocínované, průřez 6mm2 / M12","100ks",37.112499118578143,{"$f":"F1267*(1-Elteq!$F$9)","v":37.112499118578143},"8591735016548"]
["TECHNIK","OL 10-M 4",null,"Oko lehčené Cu pocínované, průřez 10mm2 / M4","100ks",25.236499400633139,{"$f":"F1268*(1-Elteq!$F$9)","v":25.236499400633139},"8591735021535"]
["TECHNIK","OL 10-M 5",null,"Oko lehčené Cu pocínované, průřez 10mm2 / M5","100ks",24.865374409447359,{"$f":"F1269*(1-Elteq!$F$9)","v":24.865374409447359},"8591735003098"]
["TECHNIK","OL 10-M 6",null,"Oko lehčené Cu pocínované, průřez 10mm2 / M6","100ks",24.865374409447359,{"$f":"F1270*(1-Elteq!$F$9)","v":24.865374409447359},"8591735003104"]
["TECHNIK","OL 10-M 8",null,"Oko lehčené Cu pocínované, průřez 10mm2 / M8","100ks",25.236499400633139,{"$f":"F1271*(1-Elteq!$F$9)","v":25.236499400633139},"8591735003111"]
["TECHNIK","OL 10-M10",null,"Oko lehčené Cu pocínované, průřez 10mm2 / M10","100ks",28.947749312490952,{"$f":"F1272*(1-Elteq!$F$9)","v":28.947749312490952},"8591735003128"]
["TECHNIK","OL 10-M12",null,"Oko lehčené Cu pocínované, průřez 10mm2 / M12","100ks",38.596999083321272,{"$f":"F1273*(1-Elteq!$F$9)","v":38.596999083321272},"8591735003135"]
["TECHNIK","OL 16-M 4",null,"Oko lehčené Cu pocínované, průřez 16mm2 / M4","100ks",51.21524878363784,{"$f":"F1274*(1-Elteq!$F$9)","v":51.21524878363784},"8591735052959"]
["TECHNIK","OL 16-M 5",null,"Oko lehčené Cu pocínované, průřez 16mm2 / M5","100ks",34.143499189091891,{"$f":"F1275*(1-Elteq!$F$9)","v":34.143499189091891},"8591735003142"]
["TECHNIK","OL 16-M 5/F",null,"Oko lehčené Cu pocínované, průřez 16mm2 / M5, pro flexibilní vodiče","100ks",53.44199873075253,{"$f":"F1276*(1-Elteq!$F$9)","v":53.44199873075253},"8591735046644"]
["TECHNIK","OL 16-M 6",null,"Oko lehčené Cu pocínované, průřez 16mm2 / M6","100ks",32.287874233162988,{"$f":"F1277*(1-Elteq!$F$9)","v":32.287874233162988},"8591735003159"]
["TECHNIK","OL 16-M 6/S",null,"Oko lehčené Cu pocínované, průřez 16mm2 / M6, s nahlížecím otvorem","100ks",53.44199873075253,{"$f":"F1278*(1-Elteq!$F$9)","v":53.44199873075253},"8591735055431"]
["TECHNIK","OL 16-M 8",null,"Oko lehčené Cu pocínované, průřez 16mm2 / M8","100ks",35.25687416264924,{"$f":"F1279*(1-Elteq!$F$9)","v":35.25687416264924},"8591735003166"]
["TECHNIK","OL 16-M 8/F",null,"Oko lehčené Cu pocínované, průřez 16mm2 / M8, pro flexibilní vodiče","100ks",55.668748677867221,{"$f":"F1280*(1-Elteq!$F$9)","v":55.668748677867221},"8591735038496"]
["TECHNIK","OL 16-M 8/S",null,"Oko lehčené Cu pocínované, průřez 16mm2 / M8, s nahlížecím otvorem","100ks",55.668748677867221,{"$f":"F1281*(1-Elteq!$F$9)","v":55.668748677867221},"8591735055448"]
["TECHNIK","OL 16-M10",null,"Oko lehčené Cu pocínované, průřez 16mm2 / M10","100ks",37.48362410976393,{"$f":"F1282*(1-Elteq!$F$9)","v":37.48362410976393},"8591735003173"]
["TECHNIK","OL 16-M12",null,"Oko lehčené Cu pocínované, průřez 16mm2 / M12","100ks",46.390623898222685,{"$f":"F1283*(1-Elteq!$F$9)","v":46.390623898222685},"8591735003180"]
["TECHNIK","OL 16-M12/S",null,"Oko lehčené Cu pocínované, průřez 16mm2 / M12, s nahlížecím otvorem","100ks",57.524373633796124,{"$f":"F1284*(1-Elteq!$F$9)","v":57.524373633796124},"8591735055493"]
["TECHNIK","OL 16-M16",null,"Oko lehčené Cu pocínované, průřez 16mm2 / M16","100ks",60.122248572096595,{"$f":"F1285*(1-Elteq!$F$9)","v":60.122248572096595},"8591735041915"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"OL 25-M 5",null,"Oko lehčené Cu pocínované, průřez 25mm2 / M5","25ks",10.948187239980554,{"$f":"F1286*(1-Elteq!$F$9)","v":10.948187239980554},"8591735029357"]
["TECHNIK","OL 25-M 6",null,"Oko lehčené Cu pocínované, průřez 25mm2 / M6 (také balení 50ks)","100ks",43.792748959922214,{"$f":"F1287*(1-Elteq!$F$9)","v":43.792748959922214},"8591735003197"]
["TECHNIK","OL 25-M 6/S",null,"Oko lehčené Cu pocínované, průřez 25mm2 / M6, s nahlížecím otvorem","100ks",74.96724821952786,{"$f":"F1288*(1-Elteq!$F$9)","v":74.96724821952786},"8591735055530"]
["TECHNIK","OL 25-M 8",null,"Oko lehčené Cu pocínované, průřez 25mm2 / M8 (také balení 50ks)","100ks",42.308248995179085,{"$f":"F1289*(1-Elteq!$F$9)","v":42.308248995179085},"8591735003203"]
["TECHNIK","OL 25-M 8/F",null,"Oko lehčené Cu pocínované, průřez 25mm2 / M8, pro flexibilní vodiče","100ks",64.575748466325976,{"$f":"F1290*(1-Elteq!$F$9)","v":64.575748466325976},"8591735047795"]
["TECHNIK","OL 25-M10",null,"Oko lehčené Cu pocínované, průřez 25mm2 / M10 (také balení 50ks)","100ks",46.390623898222685,{"$f":"F1291*(1-Elteq!$F$9)","v":46.390623898222685},"8591735003210"]
["TECHNIK","OL 25-M10/F",null,"Oko lehčené Cu pocínované, průřez 25mm2 / M10, pro flexibilní vodiče","100ks",72.554935776820273,{"$f":"F1292*(1-Elteq!$F$9)","v":72.554935776820273},"8591735054397"]
["TECHNIK","OL 25-M10/S",null,"Oko lehčené Cu pocínované, průřez 25mm2 / M10, s nahlížecím otvorem","100ks",76.451748184270983,{"$f":"F1293*(1-Elteq!$F$9)","v":76.451748184270983},"8591735055523"]
["TECHNIK","OL 25-M12",null,"Oko lehčené Cu pocínované, průřez 25mm2 / M12","50ks",24.123124427075794,{"$f":"F1294*(1-Elteq!$F$9)","v":24.123124427075794},"8591735003227"]
["TECHNIK","OL 25-M12/F",null,"Oko lehčené Cu pocínované, průřez 25mm2 / M12, pro flexibilní vodiče","25ks",19.112937046067746,{"$f":"F1295*(1-Elteq!$F$9)","v":19.112937046067746},"8591735041663"]
["TECHNIK","OL 25-M16",null,"Oko lehčené Cu pocínované, průřez 25mm2 / M16","25ks",24.123124427075794,{"$f":"F1296*(1-Elteq!$F$9)","v":24.123124427075794},"8591735031374"]
["TECHNIK","OL 35",null,"Oko lehčené Cu pocínované, průřez 35mm2 / bez otvoru","1ks",4.3792748959922214,{"$f":"F1297*(1-Elteq!$F$9)","v":4.3792748959922214},"8591735056759"]
["TECHNIK","OL 35-M 6",null,"Oko lehčené Cu pocínované, průřez 35mm2 / M6 (také balení 50ks)","100ks",59.379998589725034,{"$f":"F1298*(1-Elteq!$F$9)","v":59.379998589725034},"8591735003234"]
["TECHNIK","OL 35-M 6/F",null,"Oko lehčené Cu pocínované, průřez 35mm2 / M6, pro flexibilní vodiče","100ks",94.636872752374273,{"$f":"F1299*(1-Elteq!$F$9)","v":94.636872752374273},"8591735038489"]
["TECHNIK","OL 35-M 6/S",null,"Oko lehčené Cu pocínované, průřez 35mm2 / M6, s nahlížecím otvorem","100ks",90.554497849330673,{"$f":"F1300*(1-Elteq!$F$9)","v":90.554497849330673},"8591735055547"]
["TECHNIK","OL 35-M 8",null,"Oko lehčené Cu pocínované, průřez 35mm2 / M8 (také balení 50ks)","100ks",57.524373633796124,{"$f":"F1301*(1-Elteq!$F$9)","v":57.524373633796124},"8591735003241"]
["TECHNIK","OL 35-M 8/F",null,"Oko lehčené Cu pocínované, průřez 35mm2 / M8, pro flexibilní vodiče","100ks",94.636872752374273,{"$f":"F1302*(1-Elteq!$F$9)","v":94.636872752374273},"8591735035518"]
["TECHNIK","OL 35-M 8/S",null,"Oko lehčené Cu pocínované, průřez 35mm2 / M8, s nahlížecím otvorem","100ks",90.554497849330673,{"$f":"F1303*(1-Elteq!$F$9)","v":90.554497849330673},"8591735055554"]
["TECHNIK","OL 35-M10",null,"Oko lehčené Cu pocínované, průřez 35mm2 / M10 (také balení 50ks)","100ks",63.091248501582847,{"$f":"F1304*(1-Elteq!$F$9)","v":63.091248501582847},"8591735003258"]
["TECHNIK","OL 35-M10/S",null,"Oko lehčené Cu pocínované, průřez 35mm2 / M10, s nahlížecím otvorem","100ks",90.554497849330673,{"$f":"F1305*(1-Elteq!$F$9)","v":90.554497849330673},""]
["TECHNIK","OL 35-M12",null,"Oko lehčené Cu pocínované, průřez 35mm2 / M12 (také balení 50ks)","100ks",70.513748325298479,{"$f":"F1306*(1-Elteq!$F$9)","v":70.513748325298479},"8591735003265"]
["TECHNIK","OL 35-M12/S",null,"Oko lehčené Cu pocínované, průřez 35mm2 / M12, s nahlížecím otvorem","25ks",30.432249277234078,{"$f":"F1307*(1-Elteq!$F$9)","v":30.432249277234078},"8591735052737"]
["TECHNIK","OL 35-M14",null,"Oko lehčené Cu pocínované, průřez 35mm2 / M14","100ks",81.647498060871925,{"$f":"F1308*(1-Elteq!$F$9)","v":81.647498060871925},"8591735037628"]
["TECHNIK","OL 35-M16",null,"Oko lehčené Cu pocínované, průřez 35mm2 / M16","25ks",34.329061684684788,{"$f":"F1309*(1-Elteq!$F$9)","v":34.329061684684788},"8591735031381"]
["TECHNIK","OL 35-M20",null,"Oko lehčené Cu pocínované, průřez 35mm2 / M20","25ks",42.679373986364865,{"$f":"F1310*(1-Elteq!$F$9)","v":42.679373986364865},"8591735047061"]
["TECHNIK","OL 50-M 6",null,"Oko lehčené Cu pocínované, průřez 50mm2 / M6","25ks",21.154124497589542,{"$f":"F1311*(1-Elteq!$F$9)","v":21.154124497589542},"8591735015787"]
["TECHNIK","OL 50-M 8",null,"Oko lehčené Cu pocínované, průřez 50mm2 / M8","50ks",40.081499048064394,{"$f":"F1312*(1-Elteq!$F$9)","v":40.081499048064394},"8591735003272"]
["TECHNIK","OL 50-M 8/S",null,"Oko lehčené Cu pocínované, průřez 50mm2 / M8, s nahlížecím otvorem-balení 25ks","50ks",49.730748818894718,{"$f":"F1313*(1-Elteq!$F$9)","v":49.730748818894718},"8591735056575"]
["TECHNIK","OL 50-M10",null,"Oko lehčené Cu pocínované, průřez 50mm2 / M10","50ks",42.308248995179085,{"$f":"F1314*(1-Elteq!$F$9)","v":42.308248995179085},"8591735003289"]
["TECHNIK","OL 50-M12",null,"Oko lehčené Cu pocínované, průřez 50mm2 / M12","50ks",43.421623968736434,{"$f":"F1315*(1-Elteq!$F$9)","v":43.421623968736434},"8591735003296"]
["TECHNIK","OL 50-M12/F",null,"Oko lehčené Cu pocínované, průřez 50mm2 / M12, pro flexibilní vodiče","50ks",70.513748325298479,{"$f":"F1316*(1-Elteq!$F$9)","v":70.513748325298479},"8591735040956"]
["TECHNIK","OL 50-M12/S",null,"Oko lehčené Cu pocínované, průřez 50mm2 / M12, s nahlížecím otvorem","25ks",36.926936622985252,{"$f":"F1317*(1-Elteq!$F$9)","v":36.926936622985252},"8591735055455"]
["TECHNIK","OL 50-M16",null,"Oko lehčené Cu pocínované, průřez 50mm2 / M16","25ks",30.988936764012752,{"$f":"F1318*(1-Elteq!$F$9)","v":30.988936764012752},"8591735013233"]
["TECHNIK","OL 50-M20",null,"Oko lehčené Cu pocínované, průřez 50mm2 / M20","25ks",45.833936411444007,{"$f":"F1319*(1-Elteq!$F$9)","v":45.833936411444007},"8591735037635"]
["TECHNIK","OL 70",null,"Oko lehčené Cu pocínované, průřez 70mm2 / bez otvoru","1ks",4.824624885415159,{"$f":"F1320*(1-Elteq!$F$9)","v":4.824624885415159},"8591735056711"]
["TECHNIK","OL 70-M 6",null,"Oko lehčené Cu pocínované, průřez 70mm2 / M6","25ks",31.916749241977204,{"$f":"F1321*(1-Elteq!$F$9)","v":31.916749241977204},"8591735001964"]
["TECHNIK","OL 70-M 8",null,"Oko lehčené Cu pocínované, průřez 70mm2 / M8 (také balení 25ks)","50ks",60.307811067689485,{"$f":"F1322*(1-Elteq!$F$9)","v":60.307811067689485},"8591735003302"]
["TECHNIK","OL 70-M10",null,"Oko lehčené Cu pocínované, průřez 70mm2 / M10 (také balení 25ks)","50ks",60.307811067689485,{"$f":"F1323*(1-Elteq!$F$9)","v":60.307811067689485},"8591735003319"]
["TECHNIK","OL 70-M12",null,"Oko lehčené Cu pocínované, průřez 70mm2 / M12 (také balení 25ks)","50ks",62.905686005989956,{"$f":"F1324*(1-Elteq!$F$9)","v":62.905686005989956},"8591735003326"]
["TECHNIK","OL 70-M12/S",null,"Oko lehčené Cu pocínované, průřez 70mm2 / M12, s nahlížecím otvorem","50ks",88.69887289340177,{"$f":"F1325*(1-Elteq!$F$9)","v":88.69887289340177},"8591735055462"]
["TECHNIK","OL 70-M16",null,"Oko lehčené Cu pocínované, průřez 70mm2 / M16","25ks",45.648373915851117,{"$f":"F1326*(1-Elteq!$F$9)","v":45.648373915851117},"8591735003333"]
["TECHNIK","OL 70-M20",null,"Oko lehčené Cu pocínované, průřez 70mm2 / M20","25ks",57.153248642610343,{"$f":"F1327*(1-Elteq!$F$9)","v":57.153248642610343},"8591735049539"]
["TECHNIK","OL 95",null,"Oko lehčené Cu pocínované, průřez 95mm2 / bez otvoru","1ks",5.6039873669053,{"$f":"F1328*(1-Elteq!$F$9)","v":5.6039873669053},"8591735056728"]
["TECHNIK","OL 95-M 8",null,"Oko lehčené Cu pocínované, průřez 95mm2 / M8","25ks",36.555811631799472,{"$f":"F1329*(1-Elteq!$F$9)","v":36.555811631799472},"8591735003340"]
["TECHNIK","OL 95-M 8/F",null,"Oko lehčené Cu pocínované, průřez 95mm2 / M8, pro flexibilní vodiče","50ks",91.667872822888015,{"$f":"F1330*(1-Elteq!$F$9)","v":91.667872822888015},"8591735041908"]
["TECHNIK","OL 95-M10",null,"Oko lehčené Cu pocínované, průřez 95mm2 / M10 (také balení 25ks)","50ks",73.111623263598943,{"$f":"F1331*(1-Elteq!$F$9)","v":73.111623263598943},"8591735003357"]
["TECHNIK","OL 95-M10/S",null,"Oko lehčené Cu pocínované, průřez 95mm2 / M10, s nahlížecím otvorem","50ks",104.65724751439038,{"$f":"F1332*(1-Elteq!$F$9)","v":104.65724751439038},"8591735055479"]
["TECHNIK","OL 95-M12",null,"Oko lehčené Cu pocínované, průřez 95mm2 / M12 (také balení 25ks)","50ks",75.152810715120751,{"$f":"F1333*(1-Elteq!$F$9)","v":75.152810715120751},"8591735003364"]
["TECHNIK","OL 95-M12/S",null,"Oko lehčené Cu pocínované, průřez 95mm2 / M12, s nahlížecím otvorem","50ks",98.533685159824984,{"$f":"F1334*(1-Elteq!$F$9)","v":98.533685159824984},"8591735055486"]
["TECHNIK","OL 95-M14",null,"Oko lehčené Cu pocínované, průřez 95mm2 / M14","25ks",58.266623616167692,{"$f":"F1335*(1-Elteq!$F$9)","v":58.266623616167692},"8591735047948"]
["TECHNIK","OL 95-M16",null,"Oko lehčené Cu pocínované, průřez 95mm2 / M16 (také balení 25ks)","50ks",75.152810715120751,{"$f":"F1336*(1-Elteq!$F$9)","v":75.152810715120751},"8591735003371"]
["TECHNIK","OL 95-M16/S",null,"Oko lehčené Cu pocínované, průřez 95mm2 / M16, s nahlížecím otvorem","50ks",108.18293493065529,{"$f":"F1337*(1-Elteq!$F$9)","v":108.18293493065529},"8591735035358"]
["TECHNIK","OL 95-M20",null,"Oko lehčené Cu pocínované, průřez 95mm2 / M20","25ks",56.039873669053001,{"$f":"F1338*(1-Elteq!$F$9)","v":56.039873669053001},"8591735033439"]
["TECHNIK","OL120",null,"Oko lehčené Cu pocínované, průřez 120mm2 / bez otvoru","1ks",6.1977873528025507,{"$f":"F1339*(1-Elteq!$F$9)","v":6.1977873528025507},"8591735056735"]
["TECHNIK","OL120-M 6",null,"Oko lehčené Cu pocínované, průřez 120mm2 / M6","25ks",46.761748889408466,{"$f":"F1340*(1-Elteq!$F$9)","v":46.761748889408466},"8591735040789"]
["TECHNIK","OL120-M 8",null,"Oko lehčené Cu pocínované, průřez 120mm2 / M8","25ks",46.761748889408466,{"$f":"F1341*(1-Elteq!$F$9)","v":46.761748889408466},"8591735003388"]
["TECHNIK","OL120-M10",null,"Oko lehčené Cu pocínované, průřez 120mm2 / M10 (také balení 25ks)","50ks",89.069997884587551,{"$f":"F1342*(1-Elteq!$F$9)","v":89.069997884587551},"8591735003395"]
["TECHNIK","OL120-M12",null,"Oko lehčené Cu pocínované, průřez 120mm2 / M12 (také balení 25ks)","50ks",89.069997884587551,{"$f":"F1343*(1-Elteq!$F$9)","v":89.069997884587551},"8591735003401"]
["TECHNIK","OL120-M12/S",null,"Oko lehčené Cu pocínované, průřez 120mm2 / M12, s nahlížecím otvorem","50ks",126.18249700316569,{"$f":"F1344*(1-Elteq!$F$9)","v":126.18249700316569},"8591735055332"]
["TECHNIK","OL120-M16",null,"Oko lehčené Cu pocínované, průřez 120mm2 / M16 (také balení 25ks)","50ks",94.636872752374273,{"$f":"F1345*(1-Elteq!$F$9)","v":94.636872752374273},"8591735003418"]
["TECHNIK","OL120-M20",null,"Oko lehčené Cu pocínované, průřez 120mm2 / M20","50ks",115.04874726759225,{"$f":"F1346*(1-Elteq!$F$9)","v":115.04874726759225},"8591735015794"]
["TECHNIK","OL150",null,"Oko lehčené Cu pocínované, průřez 150mm2 / bez otvoru","1ks",8.6472122946287087,{"$f":"F1347*(1-Elteq!$F$9)","v":8.6472122946287087},"8591735056742"]
["TECHNIK","OL150-M 8",null,"Oko lehčené Cu pocínované, průřez 150mm2 / M8","10ks",30.246686781641188,{"$f":"F1348*(1-Elteq!$F$9)","v":30.246686781641188},"8591735040802"]
["TECHNIK","OL150-M10",null,"Oko lehčené Cu pocínované, průřez 150mm2 / M10","10ks",20.968562001996652,{"$f":"F1349*(1-Elteq!$F$9)","v":20.968562001996652},"8591735003425"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"OL150-M12",null,"Oko lehčené Cu pocínované, průřez 150mm2 / M12 (také balení 10ks)","25ks",52.421405004991634,{"$f":"F1350*(1-Elteq!$F$9)","v":52.421405004991634},"8591735003432"]
["TECHNIK","OL150-M16",null,"Oko lehčené Cu pocínované, průřez 150mm2 / M16","10ks",22.267499471146888,{"$f":"F1351*(1-Elteq!$F$9)","v":22.267499471146888},"8591735003449"]
["TECHNIK","OL150-M20",null,"Oko lehčené Cu pocínované, průřez 150mm2 / M20","10ks",33.030124215534549,{"$f":"F1352*(1-Elteq!$F$9)","v":33.030124215534549},"8591735051785"]
["TECHNIK","OL185-M 8",null,"Oko lehčené Cu pocínované, průřez 185mm2 / M8","10ks",28.947749312490952,{"$f":"F1353*(1-Elteq!$F$9)","v":28.947749312490952},"8591735042288"]
["TECHNIK","OL185-M10",null,"Oko lehčené Cu pocínované, průřez 185mm2 / M10","10ks",28.947749312490952,{"$f":"F1354*(1-Elteq!$F$9)","v":28.947749312490952},"8591735003456"]
["TECHNIK","OL185-M12",null,"Oko lehčené Cu pocínované, průřez 185mm2 / M12","10ks",28.947749312490952,{"$f":"F1355*(1-Elteq!$F$9)","v":28.947749312490952},"8591735003463"]
["TECHNIK","OL185-M16",null,"Oko lehčené Cu pocínované, průřez 185mm2 / M16","10ks",28.205499330119391,{"$f":"F1356*(1-Elteq!$F$9)","v":28.205499330119391},"8591735003470"]
["TECHNIK","OL185-M20",null,"Oko lehčené Cu pocínované, průřez 185mm2 / M20","50ks",166.07843355563719,{"$f":"F1357*(1-Elteq!$F$9)","v":166.07843355563719},"8591735031398"]
["TECHNIK","OL240-2xM12/25",null,"Oko lehčené Cu pocínované, průřez 240mm2 / 2xM12 rozteč 25mm","1ks",5.6039873669053,{"$f":"F1358*(1-Elteq!$F$9)","v":5.6039873669053},"8591735050184"]
["TECHNIK","OL240-M10",null,"Oko lehčené Cu pocínované, průřez 240mm2 / M10","10ks",36.741374127392362,{"$f":"F1359*(1-Elteq!$F$9)","v":36.741374127392362},"8591735003487"]
["TECHNIK","OL240-M12",null,"Oko lehčené Cu pocínované, průřez 240mm2 / M12","10ks",34.143499189091891,{"$f":"F1360*(1-Elteq!$F$9)","v":34.143499189091891},"8591735003494"]
["TECHNIK","OL240-M16",null,"Oko lehčené Cu pocínované, průřez 240mm2 / M16 (také balení 10ks)","25ks",85.358747972729731,{"$f":"F1361*(1-Elteq!$F$9)","v":85.358747972729731},"8591735003500"]
["TECHNIK","OL300-M12",null,"Oko lehčené Cu pocínované, průřez 300mm2 / M12","5ks",28.391061825712281,{"$f":"F1362*(1-Elteq!$F$9)","v":28.391061825712281},"8591735007492"]
["TECHNIK","OL300-M16",null,"Oko lehčené Cu pocínované, průřez 300mm2 / M16","5ks",28.391061825712281,{"$f":"F1363*(1-Elteq!$F$9)","v":28.391061825712281},"8591735007508"]
["TECHNIK","OL300-M20",null,"Oko lehčené Cu pocínované, průřez 300mm2 / M20","5ks",28.391061825712281,{"$f":"F1364*(1-Elteq!$F$9)","v":28.391061825712281},"8591735029289"]
["TECHNIK","OL400-M12",null,"Oko lehčené Cu pocínované, průřez 400mm2 / M12","10ks",91.296747831702234,{"$f":"F1365*(1-Elteq!$F$9)","v":91.296747831702234},"8591735015800"]
["TECHNIK","OL400-M16",null,"Oko lehčené Cu pocínované, průřez 400mm2 / M16","10ks",91.296747831702234,{"$f":"F1366*(1-Elteq!$F$9)","v":91.296747831702234},"8591735007515"]
["TECHNIK","OL400-M20",null,"Oko lehčené Cu pocínované, průřez 400mm2 / M20","10ks",86.472122946287087,{"$f":"F1367*(1-Elteq!$F$9)","v":86.472122946287087},"8591735033507"]
["TECHNIK","OL500-M12",null,"Oko lehčené Cu pocínované, průřez 500mm2 / M12","10ks",148.07887148312679,{"$f":"F1368*(1-Elteq!$F$9)","v":148.07887148312679},"8591735040741"]
["TECHNIK","OL500-M16",null,"Oko lehčené Cu pocínované, průřez 500mm2 / M16","10ks",135.46062178281022,{"$f":"F1369*(1-Elteq!$F$9)","v":135.46062178281022},"8591735007522"]
["TECHNIK","OL45R 10-M 8",null,"Oko lehčené Cu zahnuté 45° pocínované, průřez 10mm2 / M8","50ks",30.617811772826972,{"$f":"F1370*(1-Elteq!$F$9)","v":30.617811772826972},"8591735047320"]
["TECHNIK","OL45R 16-M 8",null,"Oko lehčené Cu zahnuté 45° pocínované, průřez 16mm2 / M8","50ks",39.524811561285723,{"$f":"F1371*(1-Elteq!$F$9)","v":39.524811561285723},"8591735047337"]
["TECHNIK","OL45R 25-M 8",null,"Oko lehčené Cu zahnuté 45° pocínované, průřez 25mm2 / M8","25ks",24.030343179279349,{"$f":"F1372*(1-Elteq!$F$9)","v":24.030343179279349},"8591735047344"]
["TECHNIK","OL45R 35-M 8",null,"Oko lehčené Cu zahnuté 45° pocínované, průřez 35mm2 / M8","25ks",35.813561649427911,{"$f":"F1373*(1-Elteq!$F$9)","v":35.813561649427911},"8591735047351"]
["TECHNIK","OL45R 35-M12",null,"Oko lehčené Cu zahnuté 45° pocínované, průřez 35mm2 / M12","25ks",47.689561367372917,{"$f":"F1374*(1-Elteq!$F$9)","v":47.689561367372917},"8591735031404"]
["TECHNIK","OL45R 35-M16",null,"Oko lehčené Cu zahnuté 45° pocínované, průřez 35mm2 / M16","25ks",52.143061261602298,{"$f":"F1375*(1-Elteq!$F$9)","v":52.143061261602298},"8591735031534"]
["TECHNIK","OL45R 50-M10",null,"Oko lehčené Cu zahnuté 45° pocínované, průřez 50mm2 / M10","25ks",52.143061261602298,{"$f":"F1376*(1-Elteq!$F$9)","v":52.143061261602298},"8591735047368"]
["TECHNIK","OL45R 70-M12",null,"Oko lehčené Cu zahnuté 45° pocínované, průřez 70mm2 / M12","25ks",67.730310891405111,{"$f":"F1377*(1-Elteq!$F$9)","v":67.730310891405111},"8591735037994"]
["TECHNIK","OL45R 95-M 8",null,"Oko lehčené Cu zahnuté 45° pocínované, průřez 95mm2 / M8","25ks",69.585935847334028,{"$f":"F1378*(1-Elteq!$F$9)","v":69.585935847334028},"8591735054359"]
["TECHNIK","OL45R240-M12",null,"Oko lehčené Cu zahnuté 45° pocínované, průřez 240mm2 / M12","10ks",61.606748536839724,{"$f":"F1379*(1-Elteq!$F$9)","v":61.606748536839724},"8591735053062"]
["TECHNIK","OL90R  6-M 4",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 6mm2 / M4","100ks",56.410998660238782,{"$f":"F1380*(1-Elteq!$F$9)","v":56.410998660238782},"8591735047160"]
["TECHNIK","OL90R  6-M 5",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 6mm2 / M5","100ks",56.410998660238782,{"$f":"F1381*(1-Elteq!$F$9)","v":56.410998660238782},"8591735030155"]
["TECHNIK","OL90R  6-M 6",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 6mm2 / M6 (balení 50ks)","100ks",56.410998660238782,{"$f":"F1382*(1-Elteq!$F$9)","v":56.410998660238782},"8591735027148"]
["TECHNIK","OL90R  6-M 8",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 6mm2 / M8","100ks",56.782123651424563,{"$f":"F1383*(1-Elteq!$F$9)","v":56.782123651424563},"8591735027131"]
["TECHNIK","OL90R  6-M10",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 6mm2 / M10 (balení 50ks)","100ks",56.782123651424563,{"$f":"F1384*(1-Elteq!$F$9)","v":56.782123651424563},"8591735040598"]
["TECHNIK","OL90R 10-M 5",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 10mm2 / M5","100ks",59.379998589725034,{"$f":"F1385*(1-Elteq!$F$9)","v":59.379998589725034},"8591735037604"]
["TECHNIK","OL90R 10-M 6",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 10mm2 / M6 (balení 50ks)","100ks",59.379998589725034,{"$f":"F1386*(1-Elteq!$F$9)","v":59.379998589725034},"8591735028541"]
["TECHNIK","OL90R 10-M 8",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 10mm2 / M8 (balení 50ks)","100ks",61.606748536839724,{"$f":"F1387*(1-Elteq!$F$9)","v":61.606748536839724},"8591735028558"]
["TECHNIK","OL90R 10-M10",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 10mm2 / M10","100ks",61.606748536839724,{"$f":"F1388*(1-Elteq!$F$9)","v":61.606748536839724},"8591735031541"]
["TECHNIK","OL90R 16-M 5",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 16mm2 / M5 (balení 50ks)","100ks",104.2861225232046,{"$f":"F1389*(1-Elteq!$F$9)","v":104.2861225232046},"8591735030148"]
["TECHNIK","OL90R 16-M 6",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 16mm2 / M6 (balení 50ks)","100ks",104.2861225232046,{"$f":"F1390*(1-Elteq!$F$9)","v":104.2861225232046},"8591735028565"]
["TECHNIK","OL90R 16-M 8",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 16mm2 / M8 (balení 50ks)","100ks",105.02837250557616,{"$f":"F1391*(1-Elteq!$F$9)","v":105.02837250557616},"8591735028572"]
["TECHNIK","OL90R 16-M10",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 16mm2 / M10 (balení 50ks)","100ks",105.02837250557616,{"$f":"F1392*(1-Elteq!$F$9)","v":105.02837250557616},"8591735028589"]
["TECHNIK","OL90R 16-M12",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 16mm2 / M12 (balení 50ks)","100ks",109.11074740861974,{"$f":"F1393*(1-Elteq!$F$9)","v":109.11074740861974},"8591735028596"]
["TECHNIK","OL90R 25-M 6",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 25mm2 / M6","100ks",158.09924624514289,{"$f":"F1394*(1-Elteq!$F$9)","v":158.09924624514289},"8591735028602"]
["TECHNIK","OL90R 25-M 8",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 25mm2 / M8 (balení 25ks)","100ks",158.09924624514289,{"$f":"F1395*(1-Elteq!$F$9)","v":158.09924624514289},"8591735028619"]
["TECHNIK","OL90R 25-M10",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 25mm2 / M10 (balení 25ks)","100ks",158.09924624514289,{"$f":"F1396*(1-Elteq!$F$9)","v":158.09924624514289},"8591735028626"]
["TECHNIK","OL90R 25-M12",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 25mm2 / M12 (balení 25ks)","100ks",162.92387113055807,{"$f":"F1397*(1-Elteq!$F$9)","v":162.92387113055807},"8591735028633"]
["TECHNIK","OL90R 35-M 6",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 35mm2 / M6","25ks",38.875342826710607,{"$f":"F1398*(1-Elteq!$F$9)","v":38.875342826710607},"8591735041632"]
["TECHNIK","OL90R 35-M 8",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 35mm2 / M8 (balení 25ks)","100ks",155.50137130684243,{"$f":"F1399*(1-Elteq!$F$9)","v":155.50137130684243},"8591735028640"]
["TECHNIK","OL90R 35-M10",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 35mm2 / M10 (balení 25ks)","100ks",155.50137130684243,{"$f":"F1400*(1-Elteq!$F$9)","v":155.50137130684243},"8591735026936"]
["TECHNIK","OL90R 35-M12",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 35mm2 / M12","25ks",39.339249065692833,{"$f":"F1401*(1-Elteq!$F$9)","v":39.339249065692833},"8591735031558"]
["TECHNIK","OL90R 35-M16",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 35mm2 / M16","25ks",39.339249065692833,{"$f":"F1402*(1-Elteq!$F$9)","v":39.339249065692833},"8591735052560"]
["TECHNIK","OL90R 50-M 6",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 50mm2 / M6","25ks",47.318436376187137,{"$f":"F1403*(1-Elteq!$F$9)","v":47.318436376187137},"8591735050887"]
["TECHNIK","OL90R 50-M 8",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 50mm2 / M8","25ks",47.318436376187137,{"$f":"F1404*(1-Elteq!$F$9)","v":47.318436376187137},"8591735028657"]
["TECHNIK","OL90R 50-M10",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 50mm2 / M10","25ks",47.318436376187137,{"$f":"F1405*(1-Elteq!$F$9)","v":47.318436376187137},"8591735026738"]
["TECHNIK","OL90R 50-M12",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 50mm2 / M12","25ks",48.246248854151588,{"$f":"F1406*(1-Elteq!$F$9)","v":48.246248854151588},"8591735028664"]
["TECHNIK","OL90R 50-M16",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 50mm2 / M16","25ks",55.11206119108855,{"$f":"F1407*(1-Elteq!$F$9)","v":55.11206119108855},"8591735031565"]
["TECHNIK","OL90R 70-M 8",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 70mm2 / M8","25ks",66.060248431069098,{"$f":"F1408*(1-Elteq!$F$9)","v":66.060248431069098},"8591735028671"]
["TECHNIK","OL90R 70-M10",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 70mm2 / M10","25ks",66.060248431069098,{"$f":"F1409*(1-Elteq!$F$9)","v":66.060248431069098},"8591735025519"]
["TECHNIK","OL90R 70-M12",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 70mm2 / M12","25ks",66.98806090903355,{"$f":"F1410*(1-Elteq!$F$9)","v":66.98806090903355},"8591735028688"]
["TECHNIK","OL90R 70-M16",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 70mm2 / M16","25ks",72.926060768006053,{"$f":"F1411*(1-Elteq!$F$9)","v":72.926060768006053},"8591735031572"]
["TECHNIK","OL90R 95-M 8",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 95mm2 / M8","25ks",74.59612322834208,{"$f":"F1412*(1-Elteq!$F$9)","v":74.59612322834208},"8591735039998"]
["TECHNIK","OL90R 95-M10",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 95mm2 / M10","25ks",73.297185759191834,{"$f":"F1413*(1-Elteq!$F$9)","v":73.297185759191834},"8591735025137"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"OL90R 95-M12",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 95mm2 / M12","25ks",73.297185759191834,{"$f":"F1414*(1-Elteq!$F$9)","v":73.297185759191834},"8591735029302"]
["TECHNIK","OL90R 95-M16",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 95mm2 / M16","25ks",81.276373069686144,{"$f":"F1415*(1-Elteq!$F$9)","v":81.276373069686144},"8591735034993"]
["TECHNIK","OL90R120-M 8",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 120mm2 / M8","10ks",30.803374268419862,{"$f":"F1416*(1-Elteq!$F$9)","v":30.803374268419862},"8591735052812"]
["TECHNIK","OL90R120-M10",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 120mm2 / M10","10ks",30.803374268419862,{"$f":"F1417*(1-Elteq!$F$9)","v":30.803374268419862},"8591735037826"]
["TECHNIK","OL90R120-M12",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 120mm2 / M12","25ks",77.008435671049654,{"$f":"F1418*(1-Elteq!$F$9)","v":77.008435671049654},"8591735029319"]
["TECHNIK","OL90R120-M16",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 120mm2 / M16","10ks",32.287874233162988,{"$f":"F1419*(1-Elteq!$F$9)","v":32.287874233162988},"8591735042325"]
["TECHNIK","OL90R150-M 8",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 150mm2 / M8","25ks",98.348122664232093,{"$f":"F1420*(1-Elteq!$F$9)","v":98.348122664232093},"8591735040796"]
["TECHNIK","OL90R150-M12",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 150mm2 / M12","10ks",39.339249065692833,{"$f":"F1421*(1-Elteq!$F$9)","v":39.339249065692833},"8591735053604"]
["TECHNIK","OL90R185-M12",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 185mm2 / M12","25ks",118.01774719707851,{"$f":"F1422*(1-Elteq!$F$9)","v":118.01774719707851},"8591735029326"]
["TECHNIK","OL90R240-M12",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 240mm2 / M12","10ks",49.359623827708937,{"$f":"F1423*(1-Elteq!$F$9)","v":49.359623827708937},"8591735038595"]
["TECHNIK","OL90R240-M16",null,"Oko lehčené Cu zahnuté 90° pocínované, průřez 240mm2 / M16","10ks",49.359623827708937,{"$f":"F1424*(1-Elteq!$F$9)","v":49.359623827708937},"8591735057039"]
["TECHNIK","NL  10-M 4",null,"Oko trubkové Cu s izolací nylon, průřez 10mm2 / M4","100ks",25.9787493830047,{"$f":"F1425*(1-Elteq!$F$9)","v":25.9787493830047},"8591735010843"]
["TECHNIK","NL  10-M 5",null,"Oko trubkové Cu s izolací nylon, průřez 10mm2 / M5","100ks",25.9787493830047,{"$f":"F1426*(1-Elteq!$F$9)","v":25.9787493830047},"8591735010850"]
["TECHNIK","NL  10-M 6",null,"Oko trubkové Cu s izolací nylon, průřez 10mm2 / M6","100ks",25.9787493830047,{"$f":"F1427*(1-Elteq!$F$9)","v":25.9787493830047},"8591735008406"]
["TECHNIK","NL  10-M 8",null,"Oko trubkové Cu s izolací nylon, průřez 10mm2 / M8","100ks",27.463249347747826,{"$f":"F1428*(1-Elteq!$F$9)","v":27.463249347747826},"8591735008413"]
["TECHNIK","NL  10-M10",null,"Oko trubkové Cu s izolací nylon, průřez 10mm2 / M10","100ks",31.174499259605643,{"$f":"F1429*(1-Elteq!$F$9)","v":31.174499259605643},"8591735008420"]
["TECHNIK","NL  10-M12",null,"Oko trubkové Cu s izolací nylon, průřez 10mm2 / M12","100ks",41.565999012807524,{"$f":"F1430*(1-Elteq!$F$9)","v":41.565999012807524},"8591735021351"]
["TECHNIK","NL  16-M 4",null,"Oko trubkové Cu s izolací nylon, průřez 16mm2 / M4","100ks",31.916749241977204,{"$f":"F1431*(1-Elteq!$F$9)","v":31.916749241977204},"8591735048600"]
["TECHNIK","NL  16-M 5",null,"Oko trubkové Cu s izolací nylon, průřez 16mm2 / M5","100ks",33.030124215534549,{"$f":"F1432*(1-Elteq!$F$9)","v":33.030124215534549},"8591735014339"]
["TECHNIK","NL  16-M 6",null,"Oko trubkové Cu s izolací nylon, průřez 16mm2 / M6","100ks",33.030124215534549,{"$f":"F1433*(1-Elteq!$F$9)","v":33.030124215534549},"8591735008437"]
["TECHNIK","NL  16-M 8",null,"Oko trubkové Cu s izolací nylon, průřez 16mm2 / M8","100ks",33.030124215534549,{"$f":"F1434*(1-Elteq!$F$9)","v":33.030124215534549},"8591735008444"]
["TECHNIK","NL  16-M10",null,"Oko trubkové Cu s izolací nylon, průřez 16mm2 / M10","100ks",36.741374127392362,{"$f":"F1435*(1-Elteq!$F$9)","v":36.741374127392362},"8591735008451"]
["TECHNIK","NL  16-M12",null,"Oko trubkové Cu s izolací nylon, průřez 16mm2 / M12","100ks",46.390623898222685,{"$f":"F1436*(1-Elteq!$F$9)","v":46.390623898222685},"8591735013158"]
["TECHNIK","NL  25-M 5",null,"Oko trubkové Cu s izolací nylon, průřez 25mm2 / M5","100ks",46.390623898222685,{"$f":"F1437*(1-Elteq!$F$9)","v":46.390623898222685},"8591735028695"]
["TECHNIK","NL  25-M 6",null,"Oko trubkové Cu s izolací nylon, průřez 25mm2 / M6","100ks",43.421623968736434,{"$f":"F1438*(1-Elteq!$F$9)","v":43.421623968736434},"8591735008468"]
["TECHNIK","NL  25-M 8",null,"Oko trubkové Cu s izolací nylon, průřez 25mm2 / M8","100ks",44.163873951107995,{"$f":"F1439*(1-Elteq!$F$9)","v":44.163873951107995},"8591735008475"]
["TECHNIK","NL  25-M10",null,"Oko trubkové Cu s izolací nylon, průřez 25mm2 / M10","100ks",49.730748818894718,{"$f":"F1440*(1-Elteq!$F$9)","v":49.730748818894718},"8591735013554"]
["TECHNIK","NL  25-M12",null,"Oko trubkové Cu s izolací nylon, průřez 25mm2 / M12","100ks",64.575748466325976,{"$f":"F1441*(1-Elteq!$F$9)","v":64.575748466325976},"8591735014032"]
["TECHNIK","NL  35-M 6",null,"Oko trubkové Cu s izolací nylon, průřez 5mm2 / M6","50ks",36.370249136206581,{"$f":"F1442*(1-Elteq!$F$9)","v":36.370249136206581},"8591735021368"]
["TECHNIK","NL  35-M 8",null,"Oko trubkové Cu s izolací nylon, průřez 5mm2 / M8","50ks",36.741374127392362,{"$f":"F1443*(1-Elteq!$F$9)","v":36.741374127392362},"8591735010553"]
["TECHNIK","NL  35-M10",null,"Oko trubkové Cu s izolací nylon, průřez 35mm2 / M10","50ks",38.968124074507053,{"$f":"F1444*(1-Elteq!$F$9)","v":38.968124074507053},"8591735010560"]
["TECHNIK","NL  35-M12",null,"Oko trubkové Cu s izolací nylon, průřez 35mm2 / M12","50ks",42.308248995179085,{"$f":"F1445*(1-Elteq!$F$9)","v":42.308248995179085},"8591735028701"]
["TECHNIK","NL  50-M 6",null,"Oko trubkové Cu s izolací nylon, průřez 50mm2 / M6","25ks",24.123124427075794,{"$f":"F1446*(1-Elteq!$F$9)","v":24.123124427075794},"8591735055981"]
["TECHNIK","NL  50-M 8",null,"Oko trubkové Cu s izolací nylon, průřez 50mm2 / M8","25ks",24.123124427075794,{"$f":"F1447*(1-Elteq!$F$9)","v":24.123124427075794},"8591735012625"]
["TECHNIK","NL  50-M10",null,"Oko trubkové Cu s izolací nylon, průřez 50mm2 / M10","25ks",25.236499400633139,{"$f":"F1448*(1-Elteq!$F$9)","v":25.236499400633139},"8591735013387"]
["TECHNIK","NL  50-M12",null,"Oko trubkové Cu s izolací nylon, průřez 50mm2 / M12","25ks",26.720999365376265,{"$f":"F1449*(1-Elteq!$F$9)","v":26.720999365376265},"8591735013134"]
["TECHNIK","NL  70-M 8",null,"Oko trubkové Cu s izolací nylon, průřez 70mm2 / M8","25ks",34.143499189091891,{"$f":"F1450*(1-Elteq!$F$9)","v":34.143499189091891},"8591735014049"]
["TECHNIK","NL  70-M10",null,"Oko trubkové Cu s izolací nylon, průřez 70mm2 / M10","25ks",37.48362410976393,{"$f":"F1451*(1-Elteq!$F$9)","v":37.48362410976393},"8591735008482"]
["TECHNIK","NL  70-M12",null,"Oko trubkové Cu s izolací nylon, průřez 70mm2 / M12","25ks",38.596999083321272,{"$f":"F1452*(1-Elteq!$F$9)","v":38.596999083321272},"8591735021375"]
["TECHNIK","NL  95-M 8",null,"Oko trubkové Cu s izolací nylon, průřez 95mm2 / M8","25ks",47.503998871780027,{"$f":"F1453*(1-Elteq!$F$9)","v":47.503998871780027},"8591735016555"]
["TECHNIK","NL  95-M10",null,"Oko trubkové Cu s izolací nylon, průřez 95mm2 / M10","25ks",48.988498836523149,{"$f":"F1454*(1-Elteq!$F$9)","v":48.988498836523149},"8591735010546"]
["TECHNIK","NL  95-M12",null,"Oko trubkové Cu s izolací nylon, průřez 95mm2 / M12","25ks",51.58637377482362,{"$f":"F1455*(1-Elteq!$F$9)","v":51.58637377482362},"8591735016562"]
["TECHNIK","NL 120-M10",null,"Oko trubkové Cu s izolací nylon, průřez 120mm2 / M10","25ks",75.338373210713641,{"$f":"F1456*(1-Elteq!$F$9)","v":75.338373210713641},"8591735014056"]
["TECHNIK","NL 120-M12",null,"Oko trubkové Cu s izolací nylon, průřez 120mm2 / M12","25ks",78.307373140199886,{"$f":"F1457*(1-Elteq!$F$9)","v":78.307373140199886},"8591735021382"]
["TECHNIK","NL 150-M12",null,"Oko trubkové Cu s izolací nylon, průřez 150mm2 / M12","15ks",64.575748466325976,{"$f":"F1458*(1-Elteq!$F$9)","v":64.575748466325976},"8591735019365"]
["TECHNIK","OP  6-10/2xM 6",null,"Oko příložkové Cu pocínované, průřez 6-10mm2 / 2xM6","10ks",22.824186957925559,{"$f":"F1459*(1-Elteq!$F$9)","v":22.824186957925559},"8591735012472"]
["TECHNIK","OP  6-10/2xM 8",null,"Oko příložkové Cu pocínované, průřez 6-10mm2 / 2xM8","10ks",25.236499400633139,{"$f":"F1460*(1-Elteq!$F$9)","v":25.236499400633139},"8591735019631"]
["TECHNIK","OP  6-10/2xM10",null,"Oko příložkové Cu pocínované, průřez 6-10mm2 / 2xM10","10ks",27.83437433893361,{"$f":"F1461*(1-Elteq!$F$9)","v":27.83437433893361},"8591735037130"]
["TECHNIK","OP 10-16/2xM 6",null,"Oko příložkové Cu pocínované, průřez 10-16mm2 / 2xM6","10ks",18.185124568103291,{"$f":"F1462*(1-Elteq!$F$9)","v":18.185124568103291},"8591735015817"]
["TECHNIK","OP 10-16/2xM 8",null,"Oko příložkové Cu pocínované, průřez 10-16mm2 / 2xM8","10ks",27.945711836289345,{"$f":"F1463*(1-Elteq!$F$9)","v":27.945711836289345},"8591735011314"]
["TECHNIK","OP 16-25/2xM 8",null,"Oko příložkové Cu pocínované, průřez 16-25mm2 / 2xM8","10ks",21.896374479961107,{"$f":"F1464*(1-Elteq!$F$9)","v":21.896374479961107},"8591735021610"]
["TECHNIK","OP 16-25/2xM10",null,"Oko příložkové Cu pocínované, průřez 16-25mm2 / 2xM10","10ks",32.658999224348769,{"$f":"F1465*(1-Elteq!$F$9)","v":32.658999224348769},"8591735055035"]
["TECHNIK","OP 16-25/4xM 6",null,"Oko příložkové Cu pocínované, průřez 16-25mm2 / 4xM6","10ks",64.946873457511757,{"$f":"F1466*(1-Elteq!$F$9)","v":64.946873457511757},"8591735017217"]
["TECHNIK","OP 16-25/4xM 8",null,"Oko příložkové Cu pocínované, průřez 16-25mm2 / 4xM8","10ks",46.761748889408466,{"$f":"F1467*(1-Elteq!$F$9)","v":46.761748889408466},"8591735011321"]
["TECHNIK","OP 16-25/4xM10",null,"Oko příložkové Cu pocínované, průřez 16-25mm2 / 4xM10","10ks",49.953423813606186,{"$f":"F1468*(1-Elteq!$F$9)","v":49.953423813606186},"8591735015824"]
["TECHNIK","OP 16-25/4xM12",null,"Oko příložkové Cu pocínované, průřez 16-25mm2 / 4xM12","10ks",50.101873810080498,{"$f":"F1469*(1-Elteq!$F$9)","v":50.101873810080498},""]
["TECHNIK","OP 25-35/2xM 8",null,"Oko příložkové Cu pocínované, průřez 25-35mm2 / 2xM8","10ks",23.380874444704233,{"$f":"F1470*(1-Elteq!$F$9)","v":23.380874444704233},"8591735021627"]
["TECHNIK","OP 25-35/4xM 8",null,"Oko příložkové Cu pocínované, průřez 25-35mm2 / 4xM8","10ks",47.615336369135761,{"$f":"F1471*(1-Elteq!$F$9)","v":47.615336369135761},"8591735015831"]
["TECHNIK","OP 25-35/4xM10",null,"Oko příložkové Cu pocínované, průřez 25-35mm2 / 4xM10","10ks",54.555373704309872,{"$f":"F1472*(1-Elteq!$F$9)","v":54.555373704309872},"8591735011338"]
["TECHNIK","OP 25-35/4xM12",null,"Oko příložkové Cu pocínované, průřez 25-35mm2 / 4xM12","10ks",59.751123580910814,{"$f":"F1473*(1-Elteq!$F$9)","v":59.751123580910814},"8591735049447"]
["TECHNIK","OP 35-50/4xM 8",null,"Oko příložkové Cu pocínované, průřez 35-50mm2 / 4xM8","10ks",96.121372717117396,{"$f":"F1474*(1-Elteq!$F$9)","v":96.121372717117396},"8591735021634"]
["TECHNIK","OP 35-50/4xM10",null,"Oko příložkové Cu pocínované, průřez 35-50mm2 / 4xM10","10ks",34.514624180277679,{"$f":"F1475*(1-Elteq!$F$9)","v":34.514624180277679},"8591735015848"]
["TECHNIK","OP 35-50/4xM12",null,"Oko příložkové Cu pocínované, průřez 35-50mm2 / 4xM12","10ks",69.400373351741138,{"$f":"F1476*(1-Elteq!$F$9)","v":69.400373351741138},"8591735049454"]
["TECHNIK","OP 50-70/4xM 8",null,"Oko příložkové Cu pocínované, průřez 50-70mm2 / 4xM8","10ks",78.307373140199886,{"$f":"F1477*(1-Elteq!$F$9)","v":78.307373140199886},"8591735029661"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"OP 50-70/4xM10",null,"Oko příložkové Cu pocínované, průřez 50-70mm2 / 4xM10","10ks",46.390623898222685,{"$f":"F1478*(1-Elteq!$F$9)","v":46.390623898222685},"8591735011345"]
["TECHNIK","OP 50-70/4xM12",null,"Oko příložkové Cu pocínované, průřez 50-70mm2 / 4xM12","10ks",99.090372646603655,{"$f":"F1479*(1-Elteq!$F$9)","v":99.090372646603655},"8591735021641"]
["TECHNIK","OP 70- 95/4xM10",null,"Oko příložkové Cu pocínované, průřez 70-95mm2 / 4xM10","10ks",100.57487261134678,{"$f":"F1480*(1-Elteq!$F$9)","v":100.57487261134678},"8591735011352"]
["TECHNIK","OP 70- 95/4xM12",null,"Oko příložkové Cu pocínované, průřez 70-95mm2 / 4xM12","10ks",61.235623545653944,{"$f":"F1481*(1-Elteq!$F$9)","v":61.235623545653944},"8591735015855"]
["TECHNIK","OP 70-120/4xM10",null,"Oko příložkové Cu pocínované, průřez 70-120mm2 / 4xM10","10ks",118.38887218826429,{"$f":"F1482*(1-Elteq!$F$9)","v":118.38887218826429},"8591735015862"]
["TECHNIK","OP 70-120/4xM12",null,"Oko příložkové Cu pocínované, průřez 70-120mm2 / 4xM12","10ks",82.018623052057706,{"$f":"F1483*(1-Elteq!$F$9)","v":82.018623052057706},"8591735021658"]
["TECHNIK","OP 70-120/4xM16",null,"Oko příložkové Cu pocínované, průřez 70-120mm2 / 4xM16","10ks",94.636872752374273,{"$f":"F1484*(1-Elteq!$F$9)","v":94.636872752374273},""]
["TECHNIK","OP 95-150/4xM10",null,"Oko příložkové Cu pocínované, průřez 95-150mm2 / 4xM10","10ks",127.66699696790882,{"$f":"F1485*(1-Elteq!$F$9)","v":127.66699696790882},"8591735033446"]
["TECHNIK","OP 95-150/4xM12",null,"Oko příložkové Cu pocínované, průřez 95-150mm2 / 4xM12","10ks",127.66699696790882,{"$f":"F1486*(1-Elteq!$F$9)","v":127.66699696790882},"8591735036683"]
["TECHNIK","OP 95-150/4xM16",null,"Oko příložkové Cu pocínované, průřez 95-150mm2 / 4xM16","10ks",93.894622770002712,{"$f":"F1487*(1-Elteq!$F$9)","v":93.894622770002712},"8591735027872"]
["TECHNIK","OP150-240/4xM10",null,"Oko příložkové Cu pocínované, průřez 150-240mm2 / 4xM10","10ks",169.23299598071634,{"$f":"F1488*(1-Elteq!$F$9)","v":169.23299598071634},"8591735049461"]
["TECHNIK","OP150-240/4xM12",null,"Oko příložkové Cu pocínované, průřez 150-240mm2 / 4xM12","10ks",169.23299598071634,{"$f":"F1489*(1-Elteq!$F$9)","v":169.23299598071634},"8591735021665"]
["TECHNIK","OP150-240/4xM16",null,"Oko příložkové Cu pocínované, průřez 150-240mm2 / 4xM16","10ks",178.88224575154666,{"$f":"F1490*(1-Elteq!$F$9)","v":178.88224575154666},"8591735021672"]
["TECHNIK","OP150-240/4xM20",null,"Oko příložkové Cu pocínované, průřez 150-240mm2 / 4xM20","10ks",178.88224575154666,{"$f":"F1491*(1-Elteq!$F$9)","v":178.88224575154666},"8591735037840"]
["TECHNIK","OP185-300/4xM12",null,"Oko příložkové Cu pocínované, průřez 185-300mm2 / 4xM12","10ks",173.68649587494573,{"$f":"F1492*(1-Elteq!$F$9)","v":173.68649587494573},"8591735037673"]
["TECHNIK","OI  0,5-M 2,5/PA",null,"Oko izolované, průřez 0,1-0,5mm2 / M2,5 / šíře 5mm, izolace PA","100ks",5.8637748607353473,{"$f":"F1493*(1-Elteq!$F$9)","v":5.8637748607353473},"8591735001858"]
["TECHNIK","OI  0,5-M 2/PA",null,"Oko izolované, průřez 0,1-0,5mm2 / M2 / šíře 5mm, izolace PA","100ks",5.8637748607353473,{"$f":"F1494*(1-Elteq!$F$9)","v":5.8637748607353473},"8591735001841"]
["TECHNIK","OI  0,5-M 3,5/PA",null,"Oko izolované, průřez 0,1-0,5mm2 / M3,5 / šíře 6mm, izolace PA","100ks",6.1235623545653937,{"$f":"F1495*(1-Elteq!$F$9)","v":6.1235623545653937},"8591735001872"]
["TECHNIK","OI  0,5-M 3/PA",null,"Oko izolované, průřez 0,1-0,5mm2 / M3 / šíře 5mm, izolace PA","100ks",5.7153248642610341,{"$f":"F1496*(1-Elteq!$F$9)","v":5.7153248642610341},"8591735001865"]
["TECHNIK","OI  0,5-M 4/PA",null,"Oko izolované, průřez 0,1-0,5mm2 / M4 / šíře 6,5mm, izolace PA","100ks",5.7153248642610341,{"$f":"F1497*(1-Elteq!$F$9)","v":5.7153248642610341},"8591735001889"]
["TECHNIK","OI  0,5-M 5/PA",null,"Oko izolované, průřez 0,1-0,5mm2 / M5 / šíře 8mm, izolace PA","100ks",6.0122248572096595,{"$f":"F1498*(1-Elteq!$F$9)","v":6.0122248572096595},"8591735001896"]
["TECHNIK","OI  1,5-M 2,5",null,"Oko izolované, průřez 0,5-1,5mm2 / M2,5 / šíře 6mm, izolace PVC","100ks",3.4143499189091893,{"$f":"F1499*(1-Elteq!$F$9)","v":3.4143499189091893},"8591735001919"]
["TECHNIK","OI  1,5-M 2,5/E",null,"Oko izolované, průřez 0,5-1,5mm2 / M2,5 / šíře 6mm, izolace PVC","100ks",3.6741374127392366,{"$f":"F1500*(1-Elteq!$F$9)","v":3.6741374127392366},"8591735021870"]
["TECHNIK","OI  1,5-M 3",null,"Oko izolované, průřez 0,5-1,5mm2 / M3 / šíře 6mm, izolace PVC","100ks",3.4143499189091893,{"$f":"F1501*(1-Elteq!$F$9)","v":3.4143499189091893},"8591735001926"]
["TECHNIK","OI  1,5-M 3,5",null,"Oko izolované, průřez 0,5-1,5mm2 / M3,5 / šíře 6,6mm, izolace PVC","100ks",3.4143499189091893,{"$f":"F1502*(1-Elteq!$F$9)","v":3.4143499189091893},"8591735001933"]
["TECHNIK","OI  1,5-M 3,5/E",null,"Oko izolované, průřez 0,5-1,5mm2 / M3,5 / šíře 6,6mm, izolace PVC","100ks",3.8968124074507053,{"$f":"F1503*(1-Elteq!$F$9)","v":3.8968124074507053},"8591735019792"]
["TECHNIK","OI  1,5-M 3,5/PA",null,"Oko izolované, průřez 0,5-1,5mm2 / M3,5 / šíře 6,6mm, izolace PA","100ks",6.4946873457511751,{"$f":"F1504*(1-Elteq!$F$9)","v":6.4946873457511751},"8591735027247"]
["TECHNIK","OI  1,5-M 3,5/PC",null,"Oko izolované, průřez 0,5-1,5mm2 / M3,5 / šíře 6,6mm, izolace PC","100ks",6.2720123510397068,{"$f":"F1505*(1-Elteq!$F$9)","v":6.2720123510397068},"8591735010027"]
["TECHNIK","OI  1,5-M 3/E",null,"Oko izolované, průřez 0,5-1,5mm2 / M3 / šíře 6mm, izolace PVC","100ks",3.8968124074507053,{"$f":"F1506*(1-Elteq!$F$9)","v":3.8968124074507053},"8591735017187"]
["TECHNIK","OI  1,5-M 3/PA",null,"Oko izolované, průřez 0,5-1,5mm2 / M3 / šíře 6mm, izolace PA","100ks",6.4946873457511751,{"$f":"F1507*(1-Elteq!$F$9)","v":6.4946873457511751},"8591735018740"]
["TECHNIK","OI  1,5-M 3/PC",null,"Oko izolované, průřez 0,5-1,5mm2 / M3 / šíře 6mm, izolace PC","100ks",6.2720123510397068,{"$f":"F1508*(1-Elteq!$F$9)","v":6.2720123510397068},"8591735010010"]
["TECHNIK","OI  1,5-M 3/PK",null,"Oko izolované, průřez 0,5-1,5mm2 / M3 / šíře 6mm, izolace PC","100ks",7.4596123228342073,{"$f":"F1509*(1-Elteq!$F$9)","v":7.4596123228342073},"8591735022662"]
["TECHNIK","OI  1,5-M 4",null,"Oko izolované, průřez 0,5-1,5mm2 / M4 / šíře 8mm, izolace PVC","100ks",3.4143499189091893,{"$f":"F1510*(1-Elteq!$F$9)","v":3.4143499189091893},"8591735001940"]
["TECHNIK","OI  1,5-M 4/7",null,"Oko izolované, průřez 0,5-1,5mm2 / M4 / šíře 6,8mm, izolace PVC","100ks",3.4143499189091893,{"$f":"F1511*(1-Elteq!$F$9)","v":3.4143499189091893},"8591735026646"]
["TECHNIK","OI  1,5-M 4/7/E",null,"Oko izolované, průřez 0,5-1,5mm2 / M4 / šíře 6,8mm, izolace PVC","100ks",3.8968124074507053,{"$f":"F1512*(1-Elteq!$F$9)","v":3.8968124074507053},"8591735027230"]
["TECHNIK","OI  1,5-M 4/E",null,"Oko izolované, průřez 0,5-1,5mm2 / M4 / šíře 8mm, izolace PVC","100ks",3.8968124074507053,{"$f":"F1513*(1-Elteq!$F$9)","v":3.8968124074507053},"8591735017194"]
["TECHNIK","OI  1,5-M 4/PA",null,"Oko izolované, průřez 0,5-1,5mm2 / M4 / šíře 8mm, izolace PA","100ks",6.4946873457511751,{"$f":"F1514*(1-Elteq!$F$9)","v":6.4946873457511751},"8591735018757"]
["TECHNIK","OI  1,5-M 4/PC",null,"Oko izolované, průřez 0,5-1,5mm2 / M4 / šíře 8mm, izolace PC","100ks",6.383349848395441,{"$f":"F1515*(1-Elteq!$F$9)","v":6.383349848395441},"8591735022686"]
["TECHNIK","OI  1,5-M 4/PK",null,"Oko izolované, průřez 0,5-1,5mm2 / M4 / šíře 8mm, izolace PC","100ks",7.7193998166642546,{"$f":"F1516*(1-Elteq!$F$9)","v":7.7193998166642546},"8591735022679"]
["TECHNIK","OI  1,5-M 5",null,"Oko izolované, průřez 0,5-1,5mm2 / M5 / šíře 8mm, izolace PVC","100ks",3.5627999153835019,{"$f":"F1517*(1-Elteq!$F$9)","v":3.5627999153835019},"8591735001957"]
["TECHNIK","OI  1,5-M 5/10",null,"Oko izolované, průřez 0,5-1,5mm2 / M5 / šíře 10mm, izolace PVC","100ks",3.6370249136206585,{"$f":"F1518*(1-Elteq!$F$9)","v":3.6370249136206585},"8591735022464"]
["TECHNIK","OI  1,5-M 5/10/E",null,"Oko izolované, průřez 0,5-1,5mm2 / M5 / šíře 10mm, izolace PVC","100ks",4.045262403925018,{"$f":"F1519*(1-Elteq!$F$9)","v":4.045262403925018},"8591735025106"]
["TECHNIK","OI  1,5-M 5/10/PA",null,"Oko izolované, průřez 0,5-1,5mm2 / M5 / šíře 10mm, izolace PA","100ks",6.6802498413440663,{"$f":"F1520*(1-Elteq!$F$9)","v":6.6802498413440663},"8591735028510"]
["TECHNIK","OI  1,5-M 5/10/PC",null,"Oko izolované, průřez 0,5-1,5mm2 / M5 / šíře 10mm, izolace PC","100ks",6.4946873457511751,{"$f":"F1521*(1-Elteq!$F$9)","v":6.4946873457511751},"8591735009991"]
["TECHNIK","OI  1,5-M 5/10/PK",null,"Oko izolované, průřez 0,5-1,5mm2 / M5 / šíře 10mm, izolace PC","100ks",7.9420748113757229,{"$f":"F1522*(1-Elteq!$F$9)","v":7.9420748113757229},"8591735022693"]
["TECHNIK","OI  1,5-M 5/E",null,"Oko izolované, průřez 0,5-1,5mm2 / M5 / šíře 8mm, izolace PVC","100ks",4.045262403925018,{"$f":"F1523*(1-Elteq!$F$9)","v":4.045262403925018},"8591735019808"]
["TECHNIK","OI  1,5-M 5/PA",null,"Oko izolované, průřez 0,5-1,5mm2 / M5 / šíře 8mm, izolace PA","100ks",6.6802498413440663,{"$f":"F1524*(1-Elteq!$F$9)","v":6.6802498413440663},"8591735018764"]
["TECHNIK","OI  1,5-M 6",null,"Oko izolované, průřez 0,5-1,5mm2 / M6 / šíře 11mm, izolace PVC","100ks",5.0844123792452063,{"$f":"F1525*(1-Elteq!$F$9)","v":5.0844123792452063},"8591735001971"]
["TECHNIK","OI  1,5-M 6/E",null,"Oko izolované, průřez 0,5-1,5mm2 / M6 / šíře 11mm, izolace PVC","100ks",5.5297623686681439,{"$f":"F1526*(1-Elteq!$F$9)","v":5.5297623686681439},"8591735018726"]
["TECHNIK","OI  1,5-M 6/PA",null,"Oko izolované, průřez 0,5-1,5mm2 / M6 / šíře 11mm, izolace PA","100ks",6.8658123369369566,{"$f":"F1527*(1-Elteq!$F$9)","v":6.8658123369369566},"8591735018771"]
["TECHNIK","OI  1,5-M 6/PK",null,"Oko izolované, průřez 0,5-1,5mm2 / M6 / šíře 11mm, izolace PC","100ks",9.7976997673046302,{"$f":"F1528*(1-Elteq!$F$9)","v":9.7976997673046302},"8591735022709"]
["TECHNIK","OI  1,5-M 8",null,"Oko izolované, průřez 0,5-1,5mm2 / M8 / šíře 12mm, izolace PVC","100ks",5.3813123721938307,{"$f":"F1529*(1-Elteq!$F$9)","v":5.3813123721938307},"8591735001988"]
["TECHNIK","OI  1,5-M 8/14",null,"Oko izolované, průřez 0,5-1,5mm2 / M8 / šíře 14mm, izolace PVC","100ks",5.5297623686681439,{"$f":"F1530*(1-Elteq!$F$9)","v":5.5297623686681439},"8591735018474"]
["TECHNIK","OI  1,5-M 8/14/E",null,"Oko izolované, průřez 0,5-1,5mm2 / M8 / šíře 14mm, izolace PVC","100ks",5.8637748607353473,{"$f":"F1531*(1-Elteq!$F$9)","v":5.8637748607353473},"8591735019815"]
["TECHNIK","OI  1,5-M 8/14/PA",null,"Oko izolované, průřez 0,5-1,5mm2 / M8 / šíře 14mm, izolace PA","100ks",8.7585497919844428,{"$f":"F1532*(1-Elteq!$F$9)","v":8.7585497919844428},"8591735018788"]
["TECHNIK","OI  1,5-M 8/PA",null,"Oko izolované, průřez 0,5-1,5mm2 / M8 / šíře 12mm, izolace PA","100ks",8.6472122946287087,{"$f":"F1533*(1-Elteq!$F$9)","v":8.6472122946287087},"8591735055592"]
["TECHNIK","OI  1,5-M 8/PC",null,"Oko izolované, průřez 0,5-1,5mm2 / M8 / šíře 12mm, izolace PC","100ks",8.3503123016800824,{"$f":"F1534*(1-Elteq!$F$9)","v":8.3503123016800824},"8591735010072"]
["TECHNIK","OI  1,5-M 8/PK",null,"Oko izolované, průřez 0,5-1,5mm2 / M8 / šíře 14mm, izolace PC","100ks",10.502837250557615,{"$f":"F1535*(1-Elteq!$F$9)","v":10.502837250557615},"8591735022716"]
["TECHNIK","OI  1,5-M10",null,"Oko izolované, průřez 0,5-1,5mm2 / M10 / šíře 14mm, izolace PVC","100ks",6.0864498554468156,{"$f":"F1536*(1-Elteq!$F$9)","v":6.0864498554468156},"8591735002008"]
["TECHNIK","OI  1,5-M10/18",null,"Oko izolované, průřez 0,5-1,5mm2 / M10 / šíře 18mm, izolace PVC","100ks",6.2720123510397068,{"$f":"F1537*(1-Elteq!$F$9)","v":6.2720123510397068},"8591735024963"]
["TECHNIK","OI  1,5-M10/18/E",null,"Oko izolované, průřez 0,5-1,5mm2 / M10 / šíře 18mm, izolace PVC","100ks",6.6431373422254882,{"$f":"F1538*(1-Elteq!$F$9)","v":6.6431373422254882},"8591735019822"]
["TECHNIK","OI  1,5-M10/18/PA",null,"Oko izolované, průřez 0,5-1,5mm2 / M10 / šíře 18mm, izolace PA","100ks",9.6121372717117399,{"$f":"F1539*(1-Elteq!$F$9)","v":9.6121372717117399},"8591735026639"]
["TECHNIK","OI  1,5-M10/18/PC",null,"Oko izolované, průřez 0,5-1,5mm2 / M10 / šíře 18mm, izolace PC","100ks",9.3152372787631155,{"$f":"F1540*(1-Elteq!$F$9)","v":9.3152372787631155},"8591735010089"]
["TECHNIK","OI  1,5-M10/18/PK",null,"Oko izolované, průřez 0,5-1,5mm2 / M10 / šíře 18mm, izolace PC","100ks",11.801774719707851,{"$f":"F1541*(1-Elteq!$F$9)","v":11.801774719707851},"8591735022723"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"OI  1,5-M10/E",null,"Oko izolované, průřez 0,5-1,5mm2 / M10 / šíře 14mm, izolace PVC","100ks",6.2720123510397068,{"$f":"F1542*(1-Elteq!$F$9)","v":6.2720123510397068},"8591735028480"]
["TECHNIK","OI  1,5-M12",null,"Oko izolované, průřez 0,5-1,5mm2 / M12 / šíře 18mm, izolace PVC","100ks",18.519137060170493,{"$f":"F1543*(1-Elteq!$F$9)","v":18.519137060170493},"8591735002022"]
["TECHNIK","OI  1,5-M12/E",null,"Oko izolované, průřez 0,5-1,5mm2 / M12 / šíře 18mm, izolace PVC","100ks",19.001599548712012,{"$f":"F1544*(1-Elteq!$F$9)","v":19.001599548712012},"8591735019839"]
["TECHNIK","OI  1,5-M16",null,"Oko izolované, průřez 0,5-1,5mm2 / M16 / šíře 27mm, izolace PVC","100ks",25.718961889174654,{"$f":"F1545*(1-Elteq!$F$9)","v":25.718961889174654},"8591735033644"]
["TECHNIK","OI  1,5-M20",null,"Oko izolované, průřez 0,5-1,5mm2 / M20 / šíře 27mm, izolace PVC","100ks",32.881674219060237,{"$f":"F1546*(1-Elteq!$F$9)","v":32.881674219060237},"8591735033651"]
["TECHNIK","OI  2,5-M 3",null,"Oko izolované, průřez 1,5-2,5mm2 / M3 / šíře 6mm, izolace PVC","100ks",3.7112499118578146,{"$f":"F1547*(1-Elteq!$F$9)","v":3.7112499118578146},"8591735002077"]
["TECHNIK","OI  2,5-M 3,5",null,"Oko izolované, průřez 1,5-2,5mm2 / M3,5 / šíře 6,6mm, izolace PVC","100ks",3.9339249065692834,{"$f":"F1548*(1-Elteq!$F$9)","v":3.9339249065692834},"8591735002084"]
["TECHNIK","OI  2,5-M 3,5/E",null,"Oko izolované, průřez 1,5-2,5mm2 / M3,5 / šíře 6,6mm, izolace PVC","100ks",4.2679373986364864,{"$f":"F1549*(1-Elteq!$F$9)","v":4.2679373986364864},"8591735019846"]
["TECHNIK","OI  2,5-M 3,5/PA",null,"Oko izolované, průřez 1,5-2,5mm2 / M3,5 / šíře 6,6mm, izolace PA","100ks",7.6080623193085195,{"$f":"F1550*(1-Elteq!$F$9)","v":7.6080623193085195},"8591735028527"]
["TECHNIK","OI  2,5-M 3,5/PC",null,"Oko izolované, průřez 1,5-2,5mm2 / M3,5 / šíře 6mm, izolace PC","100ks",7.6080623193085195,{"$f":"F1551*(1-Elteq!$F$9)","v":7.6080623193085195},"8591735012410"]
["TECHNIK","OI  2,5-M 3/E",null,"Oko izolované, průřez 1,5-2,5mm2 / M3 / šíře 6mm, izolace PVC","100ks",3.9710374056878615,{"$f":"F1552*(1-Elteq!$F$9)","v":3.9710374056878615},"8591735019853"]
["TECHNIK","OI  2,5-M 3/PA",null,"Oko izolované, průřez 1,5-2,5mm2 / M3 / šíře 6mm, izolace PA","100ks",6.420462347514019,{"$f":"F1553*(1-Elteq!$F$9)","v":6.420462347514019},"8591735033422"]
["TECHNIK","OI  2,5-M 3/PC",null,"Oko izolované, průřez 1,5-2,5mm2 / M3 / šíře 6mm, izolace PC","100ks",6.9771498342926916,{"$f":"F1554*(1-Elteq!$F$9)","v":6.9771498342926916},"8591735010096"]
["TECHNIK","OI  2,5-M 3/PK",null,"Oko izolované, průřez 1,5-2,5mm2 / M3 / šíře 6mm, izolace PC","100ks",8.053412308731458,{"$f":"F1555*(1-Elteq!$F$9)","v":8.053412308731458},"8591735022730"]
["TECHNIK","OI  2,5-M 4",null,"Oko izolované, průřez 1,5-2,5mm2 / M4 / šíře 8mm, izolace PVC","100ks",4.0823749030435961,{"$f":"F1556*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735002091"]
["TECHNIK","OI  2,5-M 4/7",null,"Oko izolované, průřez 1,5-2,5mm2 / M4 / šíře 6,8mm, izolace PVC","100ks",4.2308248995179083,{"$f":"F1557*(1-Elteq!$F$9)","v":4.2308248995179083},"8591735026653"]
["TECHNIK","OI  2,5-M 4/8,5",null,"Oko izolované, průřez 1,5-2,5mm2 / M4 / šíře 8,5mm, izolace PVC","100ks",4.2308248995179083,{"$f":"F1558*(1-Elteq!$F$9)","v":4.2308248995179083},"8591735046439"]
["TECHNIK","OI  2,5-M 4/E",null,"Oko izolované, průřez 1,5-2,5mm2 / M4 / šíře 8mm, izolace PVC","100ks",4.4163873951107995,{"$f":"F1559*(1-Elteq!$F$9)","v":4.4163873951107995},"8591735017996"]
["TECHNIK","OI  2,5-M 4/PA",null,"Oko izolované, průřez 1,5-2,5mm2 / M4 / šíře 8,5mm, izolace PA","100ks",7.4596123228342073,{"$f":"F1560*(1-Elteq!$F$9)","v":7.4596123228342073},"8591735018795"]
["TECHNIK","OI  2,5-M 4/PC",null,"Oko izolované, průřez 1,5-2,5mm2 / M4 / šíře 8mm, izolace PC","100ks",7.7193998166642546,{"$f":"F1561*(1-Elteq!$F$9)","v":7.7193998166642546},"8591735002107"]
["TECHNIK","OI  2,5-M 4/PK",null,"Oko izolované, průřez 1,5-2,5mm2 / M4 / šíře 8mm, izolace PC","100ks",8.5358747972729727,{"$f":"F1562*(1-Elteq!$F$9)","v":8.5358747972729727},"8591735022419"]
["TECHNIK","OI  2,5-M 5",null,"Oko izolované, průřez 1,5-2,5mm2 / M5 / šíře 10mm, izolace PVC","100ks",4.3050498977550653,{"$f":"F1563*(1-Elteq!$F$9)","v":4.3050498977550653},"8591735002114"]
["TECHNIK","OI  2,5-M 5/8",null,"Oko izolované, průřez 1,5-2,5mm2 / M5 / šíře 8mm, izolace PVC","100ks",4.4163873951107995,{"$f":"F1564*(1-Elteq!$F$9)","v":4.4163873951107995},"8591735026660"]
["TECHNIK","OI  2,5-M 5/8/E",null,"Oko izolované, průřez 1,5-2,5mm2 / M5 / šíře 8mm, izolace PVC","100ks",4.6390623898222678,{"$f":"F1565*(1-Elteq!$F$9)","v":4.6390623898222678},"8591735028497"]
["TECHNIK","OI  2,5-M 5/E",null,"Oko izolované, průřez 1,5-2,5mm2 / M5 / šíře 10mm, izolace PVC","100ks",4.6390623898222678,{"$f":"F1566*(1-Elteq!$F$9)","v":4.6390623898222678},"8591735016654"]
["TECHNIK","OI  2,5-M 5/PA",null,"Oko izolované, průřez 1,5-2,5mm2 / M5 / šíře 10mm, izolace PA","100ks",7.4596123228342073,{"$f":"F1567*(1-Elteq!$F$9)","v":7.4596123228342073},"8591735035006"]
["TECHNIK","OI  2,5-M 5/PA role",null,"Oko izolované, průřez 1,5-2,5mm2 / M5 / šíře 10mm, izolace PA (cívka)","500ks",48.506036347981635,{"$f":"F1568*(1-Elteq!$F$9)","v":48.506036347981635},"8591735040994"]
["TECHNIK","OI  2,5-M 5/PC",null,"Oko izolované, průřez 1,5-2,5mm2 / M5 / šíře 10mm, izolace PC","100ks",7.8307373140199887,{"$f":"F1569*(1-Elteq!$F$9)","v":7.8307373140199887},"8591735002121"]
["TECHNIK","OI  2,5-M 5/PK",null,"Oko izolované, průřez 1,5-2,5mm2 / M5 / šíře 10mm, izolace PC","100ks",8.7585497919844428,{"$f":"F1570*(1-Elteq!$F$9)","v":8.7585497919844428},"8591735022747"]
["TECHNIK","OI  2,5-M 6",null,"Oko izolované, průřez 1,5-2,5mm2 / M6 / šíře 11mm, izolace PVC","100ks",5.2699748748380966,{"$f":"F1571*(1-Elteq!$F$9)","v":5.2699748748380966},"8591735002138"]
["TECHNIK","OI  2,5-M 6/12/E",null,"Oko izolované, průřez 1,5-2,5mm2 / M6 / šíře 12mm, izolace PVC","100ks",5.6782123651424561,{"$f":"F1572*(1-Elteq!$F$9)","v":5.6782123651424561},"8591735040291"]
["TECHNIK","OI  2,5-M 6/E",null,"Oko izolované, průřez 1,5-2,5mm2 / M6 / šíře 11mm, izolace PVC","100ks",5.6782123651424561,{"$f":"F1573*(1-Elteq!$F$9)","v":5.6782123651424561},"8591735019105"]
["TECHNIK","OI  2,5-M 6/PA",null,"Oko izolované, průřez 1,5-2,5mm2 / M6 / šíře 12mm, izolace PA","100ks",7.8678498131385668,{"$f":"F1574*(1-Elteq!$F$9)","v":7.8678498131385668},"8591735018818"]
["TECHNIK","OI  2,5-M 6/PC",null,"Oko izolované, průřez 1,5-2,5mm2 / M6 / šíře 11mm, izolace PC","100ks",8.3131998025615044,{"$f":"F1575*(1-Elteq!$F$9)","v":8.3131998025615044},"8591735010126"]
["TECHNIK","OI  2,5-M 6/PK",null,"Oko izolované, průřez 1,5-2,5mm2 / M6 / šíře 11mm, izolace PC","100ks",9.5379122734745838,{"$f":"F1576*(1-Elteq!$F$9)","v":9.5379122734745838},"8591735022754"]
["TECHNIK","OI  2,5-M 8",null,"Oko izolované, průřez 1,5-2,5mm2 / M8 / šíře 12mm, izolace PVC","100ks",5.9751123580910814,{"$f":"F1577*(1-Elteq!$F$9)","v":5.9751123580910814},"8591735002145"]
["TECHNIK","OI  2,5-M 8/14",null,"Oko izolované, průřez 1,5-2,5mm2 / M8 / šíře 14mm, izolace PVC","100ks",5.9379998589725034,{"$f":"F1578*(1-Elteq!$F$9)","v":5.9379998589725034},"8591735021948"]
["TECHNIK","OI  2,5-M 8/14/E",null,"Oko izolované, průřez 1,5-2,5mm2 / M8 / šíře 14mm, izolace PVC","100ks",6.4946873457511751,{"$f":"F1579*(1-Elteq!$F$9)","v":6.4946873457511751},"8591735028503"]
["TECHNIK","OI  2,5-M 8/14/PA",null,"Oko izolované, průřez 1,5-2,5mm2 / M8 / šíře 14mm, izolace PA","100ks",9.4265747761188496,{"$f":"F1580*(1-Elteq!$F$9)","v":9.4265747761188496},"8591735043810"]
["TECHNIK","OI  2,5-M 8/14/PC",null,"Oko izolované, průřez 1,5-2,5mm2 / M8 / šíře 14mm, izolace PC","100ks",7.5709498201899414,{"$f":"F1581*(1-Elteq!$F$9)","v":7.5709498201899414},"8591735010133"]
["TECHNIK","OI  2,5-M 8/14/PK",null,"Oko izolované, průřez 1,5-2,5mm2 / M8 / šíře 14mm, izolace PC","100ks",10.057487261134678,{"$f":"F1582*(1-Elteq!$F$9)","v":10.057487261134678},"8591735022426"]
["TECHNIK","OI  2,5-M 8/E",null,"Oko izolované, průřez 1,5-2,5mm2 / M8 / šíře 12mm, izolace PVC","100ks",6.4946873457511751,{"$f":"F1583*(1-Elteq!$F$9)","v":6.4946873457511751},"8591735017958"]
["TECHNIK","OI  2,5-M 8/PA",null,"Oko izolované, průřez 1,5-2,5mm2 / M8 / šíře 12mm, izolace PA","100ks",9.4265747761188496,{"$f":"F1584*(1-Elteq!$F$9)","v":9.4265747761188496},"8591735018825"]
["TECHNIK","OI  2,5-M10",null,"Oko izolované, průřez 1,5-2,5mm2 / M10 / šíře 15mm, izolace PVC","100ks",6.1235623545653937,{"$f":"F1585*(1-Elteq!$F$9)","v":6.1235623545653937},"8591735002169"]
["TECHNIK","OI  2,5-M10/18",null,"Oko izolované, průřez 1,5-2,5mm2 / M10 / šíře 18mm, izolace PVC","100ks",6.1977873528025507,{"$f":"F1586*(1-Elteq!$F$9)","v":6.1977873528025507},"8591735024635"]
["TECHNIK","OI  2,5-M10/18/E",null,"Oko izolované, průřez 1,5-2,5mm2 / M10 / šíře 18mm, izolace PVC","100ks",6.3091248501582848,{"$f":"F1587*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735027087"]
["TECHNIK","OI  2,5-M10/18/PA",null,"Oko izolované, průřez 1,5-2,5mm2 / M10 / šíře 18mm, izolace PA","100ks",9.5750247725931619,{"$f":"F1588*(1-Elteq!$F$9)","v":9.5750247725931619},"8591735018832"]
["TECHNIK","OI  2,5-M10/18/PC",null,"Oko izolované, průřez 1,5-2,5mm2 / M10 / šíře 18mm, izolace PC","100ks",9.5750247725931619,{"$f":"F1589*(1-Elteq!$F$9)","v":9.5750247725931619},"8591735010140"]
["TECHNIK","OI  2,5-M10/18/PK",null,"Oko izolované, průřez 1,5-2,5mm2 / M10 / šíře 18mm, izolace PC","100ks",11.913112217063585,{"$f":"F1590*(1-Elteq!$F$9)","v":11.913112217063585},"8591735022761"]
["TECHNIK","OI  2,5-M10/E",null,"Oko izolované, průřez 1,5-2,5mm2 / M10 / šíře 15mm, izolace PVC","100ks",6.3091248501582848,{"$f":"F1591*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735019860"]
["TECHNIK","OI  2,5-M12",null,"Oko izolované, průřez 1,5-2,5mm2 / M12 / šíře 18mm, izolace PVC","100ks",10.391499753201881,{"$f":"F1592*(1-Elteq!$F$9)","v":10.391499753201881},"8591735002183"]
["TECHNIK","OI  2,5-M12/E",null,"Oko izolované, průřez 1,5-2,5mm2 / M12 / šíře 18mm, izolace PVC","100ks",10.762624744387661,{"$f":"F1593*(1-Elteq!$F$9)","v":10.762624744387661},"8591735019877"]
["TECHNIK","OI  2,5-M12/PA",null,"Oko izolované, průřez 1,5-2,5mm2 / M12 / šíře 18mm, izolace PA","100ks",10.094599760253256,{"$f":"F1594*(1-Elteq!$F$9)","v":10.094599760253256},"8591735028534"]
["TECHNIK","OI  2,5-M12/PC",null,"Oko izolované, průřez 1,5-2,5mm2 / M12 / šíře 18mm, izolace PC","100ks",10.094599760253256,{"$f":"F1595*(1-Elteq!$F$9)","v":10.094599760253256},"8591735022778"]
["TECHNIK","OI  2,5-M12/PK",null,"Oko izolované, průřez 1,5-2,5mm2 / M12 / šíře 18mm, izolace PC","100ks",12.544024702079414,{"$f":"F1596*(1-Elteq!$F$9)","v":12.544024702079414},"8591735022785"]
["TECHNIK","OI  2,5-M16",null,"Oko izolované, průřez 1,5-2,5mm2 / M16 / šíře 27mm, izolace PVC","100ks",25.681849390056076,{"$f":"F1597*(1-Elteq!$F$9)","v":25.681849390056076},"8591735033668"]
["TECHNIK","OI  2,5-M20",null,"Oko izolované, průřez 1,5-2,5mm2 / M20 / šíře 27mm, izolace PVC","100ks",33.438361705838908,{"$f":"F1598*(1-Elteq!$F$9)","v":33.438361705838908},"8591735033675"]
["TECHNIK","OI  6-M 3",null,"Oko izolované, průřez 4-6mm2 / M3 / šíře 7,2mm, izolace PVC","100ks",6.8658123369369566,{"$f":"F1599*(1-Elteq!$F$9)","v":6.8658123369369566},"8591735002190"]
["TECHNIK","OI  6-M 3,5",null,"Oko izolované, průřez 4-6mm2 / M3,5 / šíře 7,2mm, izolace PVC","100ks",9.3152372787631155,{"$f":"F1600*(1-Elteq!$F$9)","v":9.3152372787631155},"8591735002206"]
["TECHNIK","OI  6-M 3,5/E",null,"Oko izolované, průřez 4-6mm2 / M3,5 / šíře 7,2mm, izolace PVC","100ks",9.7605872681860522,{"$f":"F1601*(1-Elteq!$F$9)","v":9.7605872681860522},"8591735019884"]
["TECHNIK","OI  6-M 3,5/PC",null,"Oko izolované, průřez 4-6mm2 / M3,5 / šíře 7,2mm, izolace PC","100ks",9.9090372646603644,{"$f":"F1602*(1-Elteq!$F$9)","v":9.9090372646603644},"8591735012434"]
["TECHNIK","OI  6-M 3/E",null,"Oko izolované, průřez 4-6mm2 / M3 / šíře 7,2mm, izolace PVC","100ks",7.3482748254784731,{"$f":"F1603*(1-Elteq!$F$9)","v":7.3482748254784731},"8591735019891"]
["TECHNIK","OI  6-M 3/PA",null,"Oko izolované, průřez 4-6mm2 / M3 / šíře 7,2mm, izolace PA","100ks",9.7605872681860522,{"$f":"F1604*(1-Elteq!$F$9)","v":9.7605872681860522},"8591735040581"]
["TECHNIK","OI  6-M 3/PC",null,"Oko izolované, průřez 4-6mm2 / M3 / šíře 7,2mm, izolace PC","100ks",9.5379122734745838,{"$f":"F1605*(1-Elteq!$F$9)","v":9.5379122734745838},"8591735012427"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"OI  6-M 4",null,"Oko izolované, průřez 4-6mm2 / M4 / šíře 9,5mm, izolace PVC","100ks",7.19982482900416,{"$f":"F1606*(1-Elteq!$F$9)","v":7.19982482900416},"8591735002213"]
["TECHNIK","OI  6-M 4/7",null,"Oko izolované, průřez 4-6mm2 / M4 / šíře 7,2mm, izolace PVC","100ks",7.3482748254784731,{"$f":"F1607*(1-Elteq!$F$9)","v":7.3482748254784731},"8591735026677"]
["TECHNIK","OI  6-M 4/7/E",null,"Oko izolované, průřez 4-6mm2 / M4 / šíře 7,2mm, izolace PVC","100ks",7.8307373140199887,{"$f":"F1608*(1-Elteq!$F$9)","v":7.8307373140199887},"8591735027063"]
["TECHNIK","OI  6-M 4/8",null,"Oko izolované, průřez 4-6mm2 / M4 / šíře 8mm, izolace PVC","100ks",7.3482748254784731,{"$f":"F1609*(1-Elteq!$F$9)","v":7.3482748254784731},"8591735026684"]
["TECHNIK","OI  6-M 4/8/E",null,"Oko izolované, průřez 4-6mm2 / M4 / šíře 8mm, izolace PVC","100ks",7.8307373140199887,{"$f":"F1610*(1-Elteq!$F$9)","v":7.8307373140199887},"8591735027100"]
["TECHNIK","OI  6-M 4/E",null,"Oko izolované, průřez 4-6mm2 / M4 / šíře 9,5mm, izolace PVC","100ks",7.8307373140199887,{"$f":"F1611*(1-Elteq!$F$9)","v":7.8307373140199887},"8591735019907"]
["TECHNIK","OI  6-M 4/PA",null,"Oko izolované, průřez 4-6mm2 / M4 / šíře 9,5mm, izolace PA","100ks",9.7234747690674741,{"$f":"F1612*(1-Elteq!$F$9)","v":9.7234747690674741},"8591735018849"]
["TECHNIK","OI  6-M 4/PC",null,"Oko izolované, průřez 4-6mm2 / M4 / šíře 8mm, izolace PC","100ks",9.7976997673046302,{"$f":"F1613*(1-Elteq!$F$9)","v":9.7976997673046302},"8591735010157"]
["TECHNIK","OI  6-M 4/PK",null,"Oko izolované, průřez 4-6mm2 / M4 / šíře 8mm, izolace PC","100ks",13.954299668585383,{"$f":"F1614*(1-Elteq!$F$9)","v":13.954299668585383},"8591735022792"]
["TECHNIK","OI  6-M 5",null,"Oko izolované, průřez 4-6mm2 / M5 / šíře 10mm, izolace PVC","100ks",7.4596123228342073,{"$f":"F1615*(1-Elteq!$F$9)","v":7.4596123228342073},"8591735002220"]
["TECHNIK","OI  6-M 5/E",null,"Oko izolované, průřez 4-6mm2 / M5 / šíře 10mm, izolace PVC","100ks",7.9420748113757229,{"$f":"F1616*(1-Elteq!$F$9)","v":7.9420748113757229},"8591735017866"]
["TECHNIK","OI  6-M 5/PA",null,"Oko izolované, průřez 4-6mm2 / M5 / šíře 10mm, izolace PA","100ks",9.7234747690674741,{"$f":"F1617*(1-Elteq!$F$9)","v":9.7234747690674741},"8591735018856"]
["TECHNIK","OI  6-M 5/PC",null,"Oko izolované, průřez 4-6mm2 / M5 / šíře 10mm, izolace PC","100ks",10.205937257608991,{"$f":"F1618*(1-Elteq!$F$9)","v":10.205937257608991},"8591735010164"]
["TECHNIK","OI  6-M 5/PK",null,"Oko izolované, průřez 4-6mm2 / M5 / šíře 10mm, izolace PC","100ks",14.176974663296852,{"$f":"F1619*(1-Elteq!$F$9)","v":14.176974663296852},"8591735022808"]
["TECHNIK","OI  6-M 6",null,"Oko izolované, průřez 4-6mm2 / M6 / šíře 11mm, izolace PVC","100ks",7.9420748113757229,{"$f":"F1620*(1-Elteq!$F$9)","v":7.9420748113757229},"8591735002237"]
["TECHNIK","OI  6-M 6/E",null,"Oko izolované, průřez 4-6mm2 / M6 / šíře 11mm, izolace PVC","100ks",8.4616497990358166,{"$f":"F1621*(1-Elteq!$F$9)","v":8.4616497990358166},"8591735017545"]
["TECHNIK","OI  6-M 6/PA",null,"Oko izolované, průřez 4-6mm2 / M6 / šíře 11mm, izolace PA","100ks",9.7605872681860522,{"$f":"F1622*(1-Elteq!$F$9)","v":9.7605872681860522},"8591735018276"]
["TECHNIK","OI  6-M 6/PC",null,"Oko izolované, průřez 4-6mm2 / M6 / šíře 11mm, izolace PC","100ks",9.9090372646603644,{"$f":"F1623*(1-Elteq!$F$9)","v":9.9090372646603644},"8591735010171"]
["TECHNIK","OI  6-M 6/PK",null,"Oko izolované, průřez 4-6mm2 / M6 / šíře 11mm, izolace PC","100ks",14.436762157126898,{"$f":"F1624*(1-Elteq!$F$9)","v":14.436762157126898},"8591735022815"]
["TECHNIK","OI  6-M 8",null,"Oko izolované, průřez 4-6mm2 / M8 / šíře 14mm, izolace PVC","100ks",10.020374762016099,{"$f":"F1625*(1-Elteq!$F$9)","v":10.020374762016099},"8591735002251"]
["TECHNIK","OI  6-M 8/E",null,"Oko izolované, průřez 4-6mm2 / M8 / šíře 14mm, izolace PVC","100ks",10.651287247031927,{"$f":"F1626*(1-Elteq!$F$9)","v":10.651287247031927},"8591735019914"]
["TECHNIK","OI  6-M 8/PA",null,"Oko izolované, průřez 4-6mm2 / M8 / šíře 14mm, izolace PA","100ks",10.836849742624819,{"$f":"F1627*(1-Elteq!$F$9)","v":10.836849742624819},"8591735018283"]
["TECHNIK","OI  6-M 8/PK",null,"Oko izolované, průřez 4-6mm2 / M8 / šíře 14mm, izolace PC","100ks",17.44287458573173,{"$f":"F1628*(1-Elteq!$F$9)","v":17.44287458573173},"8591735022433"]
["TECHNIK","OI  6-M10",null,"Oko izolované, průřez 4-6mm2 / M10 / šíře 15mm, izolace PVC","100ks",10.094599760253256,{"$f":"F1629*(1-Elteq!$F$9)","v":10.094599760253256},"8591735002268"]
["TECHNIK","OI  6-M10/18",null,"Oko izolované, průřez 4-6mm2 / M10 / šíře 18mm, izolace PVC","100ks",10.205937257608991,{"$f":"F1630*(1-Elteq!$F$9)","v":10.205937257608991},"8591735021849"]
["TECHNIK","OI  6-M10/18/E",null,"Oko izolované, průřez 4-6mm2 / M10 / šíře 18mm, izolace PVC","100ks",10.762624744387661,{"$f":"F1631*(1-Elteq!$F$9)","v":10.762624744387661},"8591735027117"]
["TECHNIK","OI  6-M10/18/PA",null,"Oko izolované, průřez 4-6mm2 / M10 / šíře 18mm, izolace PA","100ks",13.546062178281023,{"$f":"F1632*(1-Elteq!$F$9)","v":13.546062178281023},"8591735018863"]
["TECHNIK","OI  6-M10/18/PC",null,"Oko izolované, průřez 4-6mm2 / M10 / šíře 18mm, izolace PC","100ks",13.063599689739508,{"$f":"F1633*(1-Elteq!$F$9)","v":13.063599689739508},"8591735010195"]
["TECHNIK","OI  6-M10/18/PK",null,"Oko izolované, průřez 4-6mm2 / M10 / šíře 18mm, izolace PC","100ks",17.81399957691751,{"$f":"F1634*(1-Elteq!$F$9)","v":17.81399957691751},"8591735022822"]
["TECHNIK","OI  6-M10/E",null,"Oko izolované, průřez 4-6mm2 / M10 / šíře 15mm, izolace PVC","100ks",10.762624744387661,{"$f":"F1635*(1-Elteq!$F$9)","v":10.762624744387661},"8591735019921"]
["TECHNIK","OI  6-M12",null,"Oko izolované, průřez 4-6mm2 / M12 / šíře 19mm, izolace PVC","100ks",12.98937469150235,{"$f":"F1636*(1-Elteq!$F$9)","v":12.98937469150235},"8591735002282"]
["TECHNIK","OI  6-M12/E",null,"Oko izolované, průřez 4-6mm2 / M12 / šíře 19mm, izolace PVC","100ks",13.546062178281023,{"$f":"F1637*(1-Elteq!$F$9)","v":13.546062178281023},"8591735019938"]
["TECHNIK","OI  6-M12/PA",null,"Oko izolované, průřez 4-6mm2 / M12 / šíře 19mm, izolace PA","100ks",14.993449643905571,{"$f":"F1638*(1-Elteq!$F$9)","v":14.993449643905571},"8591735036546"]
["TECHNIK","OI  6-M12/PK",null,"Oko izolované, průřez 4-6mm2 / M12 / šíře 19mm, izolace PC","100ks",22.304611970265466,{"$f":"F1639*(1-Elteq!$F$9)","v":22.304611970265466},"8591735022839"]
["TECHNIK","OI  6-M16",null,"Oko izolované, průřez 4-6mm2 / M16 / šíře 24mm, izolace PVC","100ks",21.710811984368217,{"$f":"F1640*(1-Elteq!$F$9)","v":21.710811984368217},"8591735002299"]
["TECHNIK","OI  6-M16/32",null,"Oko izolované, průřez 4-6mm2 / M16 / šíře 32mm, izolace PVC","100ks",38.485661585965538,{"$f":"F1641*(1-Elteq!$F$9)","v":38.485661585965538},"8591735033774"]
["TECHNIK","OI  6-M16/PA",null,"Oko izolované, průřez 4-6mm2 / M16 / šíře 32mm, izolace PA","100ks",53.44199873075253,{"$f":"F1642*(1-Elteq!$F$9)","v":53.44199873075253},"8591735055578"]
["TECHNIK","OI  6-M20",null,"Oko izolované, průřez 4-6mm2 / M20 / šíře 32mm, izolace PVC","100ks",44.163873951107995,{"$f":"F1643*(1-Elteq!$F$9)","v":44.163873951107995},"8591735033682"]
["TECHNIK","OI 10-M 5/PA",null,"Oko izolované, průřez 10mm2 / M5 / šíře 10mm, izolace PA červená","100ks",13.397612181806711,{"$f":"F1644*(1-Elteq!$F$9)","v":13.397612181806711},"8591735015688"]
["TECHNIK","OI 10-M 6/PA",null,"Oko izolované, průřez 10mm2 / M6 / šíře 11mm, izolace PA červená","100ks",15.99548712010718,{"$f":"F1645*(1-Elteq!$F$9)","v":15.99548712010718},"8591735015695"]
["TECHNIK","OI 10-M 8/PA",null,"Oko izolované, průřez 10mm2 / M8 / šíře 14mm, izolace PA červená","100ks",15.99548712010718,{"$f":"F1646*(1-Elteq!$F$9)","v":15.99548712010718},"8591735007263"]
["TECHNIK","OI 10-M10/PA",null,"Oko izolované, průřez 10mm2 / M10 / šíře 18mm, izolace PA červená","100ks",17.962449573391822,{"$f":"F1647*(1-Elteq!$F$9)","v":17.962449573391822},"8591735015701"]
["TECHNIK","OI 10-M12/PA",null,"Oko izolované, průřez 10mm2 / M12 / šíře 22mm, izolace PA červená","100ks",26.943674360087734,{"$f":"F1648*(1-Elteq!$F$9)","v":26.943674360087734},"8591735031459"]
["TECHNIK","OI 16-M 5/PA",null,"Oko izolované, průřez 16mm2 / M5 / šíře 11mm, izolace PA modrá","100ks",18.370687063696181,{"$f":"F1649*(1-Elteq!$F$9)","v":18.370687063696181},"8591735015718"]
["TECHNIK","OI 16-M 6/PA",null,"Oko izolované, průřez 16mm2 / M6 / šíře 11mm, izolace PA modrá","100ks",20.040749524032197,{"$f":"F1650*(1-Elteq!$F$9)","v":20.040749524032197},"8591735015725"]
["TECHNIK","OI 16-M 8/PA",null,"Oko izolované, průřez 16mm2 / M8 / šíře 14mm, izolace PA modrá","100ks",21.451024490538167,{"$f":"F1651*(1-Elteq!$F$9)","v":21.451024490538167},"8591735015732"]
["TECHNIK","OI 16-M10/PA",null,"Oko izolované, průřez 16mm2 / M10 / šíře 18mm, izolace PA modrá","100ks",24.716924412973047,{"$f":"F1652*(1-Elteq!$F$9)","v":24.716924412973047},"8591735015749"]
["TECHNIK","OI 16-M12/PA",null,"Oko izolované, průřez 16mm2 / M12 / šíře 22mm, izolace PA modrá","100ks",29.24464930543958,{"$f":"F1653*(1-Elteq!$F$9)","v":29.24464930543958},"8591735031466"]
["TECHNIK","OI 25-M 5/PA",null,"Oko izolované, průřez 25mm2 / M5 / šíře 12mm, izolace PA žlutá","100ks",32.881674219060237,{"$f":"F1654*(1-Elteq!$F$9)","v":32.881674219060237},"8591735031473"]
["TECHNIK","OI 25-M 6/PA",null,"Oko izolované, průřez 25mm2 / M6 / šíře 12mm, izolace PA žlutá","100ks",32.881674219060237,{"$f":"F1655*(1-Elteq!$F$9)","v":32.881674219060237},"8591735031480"]
["TECHNIK","OI 25-M 8/PA",null,"Oko izolované, průřez 25mm2 / M8 / šíře 16mm, izolace PA žlutá","100ks",35.479549157360708,{"$f":"F1656*(1-Elteq!$F$9)","v":35.479549157360708},"8591735031497"]
["TECHNIK","OI 25-M10/PA",null,"Oko izolované, průřez 25mm2 / M10 / šíře 18mm, izolace PA žlutá","100ks",39.599036559522879,{"$f":"F1657*(1-Elteq!$F$9)","v":39.599036559522879},"8591735031503"]
["TECHNIK","OI 25-M12/PA",null,"Oko izolované, průřez 25mm2 / M12 / šíře 22mm, izolace PA žlutá","100ks",46.984423884119934,{"$f":"F1658*(1-Elteq!$F$9)","v":46.984423884119934},"8591735031510"]
["TECHNIK","OI 25-M16/PA",null,"Oko izolované, průřez 25mm2 / M16 / šíře 28mm, izolace PA žlutá","100ks",58.415073612642004,{"$f":"F1659*(1-Elteq!$F$9)","v":58.415073612642004},"8591735031527"]
["TECHNIK","OI 35-M 8/PA",null,"Oko izolované, průřez 35mm2 / M8 / šíře 16mm, izolace PA červená","100ks",39.524811561285723,{"$f":"F1660*(1-Elteq!$F$9)","v":39.524811561285723},"8591735033392"]
["TECHNIK","OI 35-M10/PA",null,"Oko izolované, průřez 35mm2 / M10 / šíře 18mm, izolace PA červená","100ks",42.864936481957756,{"$f":"F1661*(1-Elteq!$F$9)","v":42.864936481957756},"8591735033354"]
["TECHNIK","OI 35-M12/PA",null,"Oko izolované, průřez 35mm2 / M12 / šíře 22mm, izolace PA červená","100ks",51.289473781874996,{"$f":"F1662*(1-Elteq!$F$9)","v":51.289473781874996},"8591735033408"]
["TECHNIK","OI 50-M 8/PA",null,"Oko izolované, průřez 50mm2 / M8 / šíře 18mm, izolace PA modrá","100ks",69.029248360555357,{"$f":"F1663*(1-Elteq!$F$9)","v":69.029248360555357},"8591735033378"]
["TECHNIK","OI 50-M10/PA",null,"Oko izolované, průřez 50mm2 / M10 / šíře 18mm, izolace PA modrá","100ks",69.029248360555357,{"$f":"F1664*(1-Elteq!$F$9)","v":69.029248360555357},"8591735033385"]
["TECHNIK","OI 50-M12/PA",null,"Oko izolované, průřez 50mm2 / M12 / šíře 22mm, izolace PA modrá","100ks",89.812247866959112,{"$f":"F1665*(1-Elteq!$F$9)","v":89.812247866959112},"8591735033361"]
["TECHNIK","OI 95-M10/PA",null,"Oko izolované, průřez 95mm2 / M10 / šíře 24mm, izolace PA červená","100ks",140.2852466682254,{"$f":"F1666*(1-Elteq!$F$9)","v":140.2852466682254},"8591735036973"]
["TECHNIK","OF 22-M 8",null,"Oko neizolované praporkové Cu stáčené z plechu, průřez 22mm2 / M8","100ks",127.29587197672303,{"$f":"F1667*(1-Elteq!$F$9)","v":127.29587197672303},"8591735055127"]
["TECHNIK","OF 38-M 8",null,"Oko neizolované praporkové Cu stáčené z plechu, průřez 38mm2 / M8","100ks",154.75912132447087,{"$f":"F1668*(1-Elteq!$F$9)","v":154.75912132447087},"8591735055110"]
["TECHNIK","OF 70-M 8",null,"Oko neizolované praporkové Cu stáčené z plechu, průřez 70mm2 / M8","100ks",282.42611829237967,{"$f":"F1669*(1-Elteq!$F$9)","v":282.42611829237967},"8591735055134"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"ON  0,5-M 2",null,"Oko neizolované Cu stáčené z plechu, průřez 0,25-0,5mm2 / M2 / šíře 5mm, dle DIN 46234","100ks",1.3360499682688132,{"$f":"F1670*(1-Elteq!$F$9)","v":1.3360499682688132},"8591735002305"]
["TECHNIK","ON  0,5-M 2,5",null,"Oko neizolované Cu stáčené z plechu, průřez 0,25-0,5mm2 / M2,5 / šíře 5mm, dle DIN 46234","100ks",1.5587249629802822,{"$f":"F1671*(1-Elteq!$F$9)","v":1.5587249629802822},"8591735002312"]
["TECHNIK","ON  0,5-M 3",null,"Oko neizolované Cu stáčené z plechu, průřez 0,25-0,5mm2 / M3 / šíře 5mm, dle DIN 46234","100ks",1.3360499682688132,{"$f":"F1672*(1-Elteq!$F$9)","v":1.3360499682688132},"8591735002329"]
["TECHNIK","ON  0,5-M 3,5",null,"Oko neizolované Cu stáčené z plechu, průřez 0,25-0,5mm2 / M3,5 / šíře 6mm, dle DIN 46234","100ks",1.5587249629802822,{"$f":"F1673*(1-Elteq!$F$9)","v":1.5587249629802822},"8591735002336"]
["TECHNIK","ON  0,5-M 4",null,"Oko neizolované Cu stáčené z plechu, průřez 0,25-0,5mm2 / M4 / šíře 6,5mm, dle DIN 46234","100ks",1.5587249629802822,{"$f":"F1674*(1-Elteq!$F$9)","v":1.5587249629802822},"8591735002343"]
["TECHNIK","ON  0,5-M 5",null,"Oko neizolované Cu stáčené z plechu, průřez 0,25-0,5mm2 / M5 / šíře 8mm","100ks",1.6700624603360166,{"$f":"F1675*(1-Elteq!$F$9)","v":1.6700624603360166},"8591735002350"]
["TECHNIK","ON  1,5-M 2",null,"Oko neizolované Cu stáčené z plechu, průřez 0,5-1,5mm2 / M2 / šíře 6mm","100ks",2.9318874303676736,{"$f":"F1676*(1-Elteq!$F$9)","v":2.9318874303676736},"8591735049508"]
["TECHNIK","ON  1,5-M 2,5",null,"Oko neizolované Cu stáčené z plechu, průřez 0,5-1,5mm2 / M2,5 / šíře 6mm, dle DIN 46234","100ks",2.9689999294862517,{"$f":"F1677*(1-Elteq!$F$9)","v":2.9689999294862517},"8591735002374"]
["TECHNIK","ON  1,5-M 3",null,"Oko neizolované Cu stáčené z plechu, průřez 0,5-1,5mm2 / M3 / šíře 6mm","100ks",2.041187451521798,{"$f":"F1678*(1-Elteq!$F$9)","v":2.041187451521798},"8591735002381"]
["TECHNIK","ON  1,5-M 3,5",null,"Oko neizolované Cu stáčené z plechu, průřez 0,5-1,5mm2 / M3,5 / šíře 6mm, dle DIN 46234","100ks",2.9318874303676736,{"$f":"F1679*(1-Elteq!$F$9)","v":2.9318874303676736},"8591735002398"]
["TECHNIK","ON  1,5-M 4",null,"Oko neizolované Cu stáčené z plechu, průřez 0,5-1,5mm2 / M4 / šíře 8mm, dle DIN 46234","100ks",2.3751999435890014,{"$f":"F1680*(1-Elteq!$F$9)","v":2.3751999435890014},"8591735002404"]
["TECHNIK","ON  1,5-M 5",null,"Oko neizolované Cu stáčené z plechu, průřez 0,5-1,5mm2 / M5 / šíře 10mm, dle DIN 46234","100ks",2.9318874303676736,{"$f":"F1681*(1-Elteq!$F$9)","v":2.9318874303676736},"8591735002411"]
["TECHNIK","ON  1,5-M 5/8",null,"Oko neizolované Cu stáčené z plechu, průřez 0,5-1,5mm2 / M5 / šíře 8mm","100ks",2.9318874303676736,{"$f":"F1682*(1-Elteq!$F$9)","v":2.9318874303676736},"8591735022488"]
["TECHNIK","ON  1,5-M 6",null,"Oko neizolované Cu stáčené z plechu, průřez 0,5-1,5mm2 / M6 / šíře 11mm","100ks",3.0061124286048297,{"$f":"F1683*(1-Elteq!$F$9)","v":3.0061124286048297},"8591735002435"]
["TECHNIK","ON  1,5-M 8",null,"Oko neizolované Cu stáčené z plechu, průřez 0,5-1,5mm2 / M8 / šíře 14mm","100ks",4.3421623968736434,{"$f":"F1684*(1-Elteq!$F$9)","v":4.3421623968736434},"8591735002442"]
["TECHNIK","ON  1,5-M10",null,"Oko neizolované Cu stáčené z plechu, průřez 0,5-1,5mm2 / M10 / šíře 18mm","100ks",5.4555373704309877,{"$f":"F1685*(1-Elteq!$F$9)","v":5.4555373704309877},"8591735002459"]
["TECHNIK","ON  1,5-M12",null,"Oko neizolované Cu stáčené z plechu, průřez 0,5-1,5mm2 / M12 / šíře 19mm","100ks",11.319312231166334,{"$f":"F1686*(1-Elteq!$F$9)","v":11.319312231166334},"8591735002466"]
["TECHNIK","ON  1,5-M16",null,"Oko neizolované Cu stáčené z plechu, průřez 0,5-1,5mm2 / M16 / šíře 27mm","100ks",20.671662009048028,{"$f":"F1687*(1-Elteq!$F$9)","v":20.671662009048028},"8591735033972"]
["TECHNIK","ON  1,5-M20",null,"Oko neizolované Cu stáčené z plechu, průřez 0,5-1,5mm2 / M20 / šíře 27mm","100ks",28.353949326593703,{"$f":"F1688*(1-Elteq!$F$9)","v":28.353949326593703},"8591735033989"]
["TECHNIK","ON  2,5-M 3",null,"Oko neizolované Cu stáčené z plechu, průřez 1,5-2,5mm2 / M3 / šíře 6mm, dle DIN 46234","100ks",2.5236499400633141,{"$f":"F1689*(1-Elteq!$F$9)","v":2.5236499400633141},"8591735002473"]
["TECHNIK","ON  2,5-M 3,5",null,"Oko neizolované Cu stáčené z plechu, průřez 1,5-2,5mm2 / M3,5 / šíře 6mm, dle DIN 46234","100ks",2.783437433893361,{"$f":"F1690*(1-Elteq!$F$9)","v":2.783437433893361},"8591735002480"]
["TECHNIK","ON  2,5-M 4",null,"Oko neizolované Cu stáčené z plechu, průřez 1,5-2,5mm2 / M4 / šíře 8mm, dle DIN 46234","100ks",2.6720999365376263,{"$f":"F1691*(1-Elteq!$F$9)","v":2.6720999365376263},"8591735002497"]
["TECHNIK","ON  2,5-M 5",null,"Oko neizolované Cu stáčené z plechu, průřez 1,5-2,5mm2 / M5 / šíře 10mm, dle DIN 46234","100ks",3.1545624250791424,{"$f":"F1692*(1-Elteq!$F$9)","v":3.1545624250791424},"8591735002503"]
["TECHNIK","ON  2,5-M 6",null,"Oko neizolované Cu stáčené z plechu, průřez 1,5-2,5mm2 / M6 / šíře 11mm, dle DIN 46234","100ks",3.4885749171463458,{"$f":"F1693*(1-Elteq!$F$9)","v":3.4885749171463458},"8591735002527"]
["TECHNIK","ON  2,5-M 8",null,"Oko neizolované Cu stáčené z plechu, průřez 1,5-2,5mm2 / M8 / šíře 14mm, dle DIN 46234","100ks",4.7875123862965809,{"$f":"F1694*(1-Elteq!$F$9)","v":4.7875123862965809},"8591735025113"]
["TECHNIK","ON  2,5-M 8/12",null,"Oko neizolované Cu stáčené z plechu, průřez 1,5-2,5mm2 / M8 / šíře 12mm","100ks",4.7875123862965809,{"$f":"F1695*(1-Elteq!$F$9)","v":4.7875123862965809},"8591735002534"]
["TECHNIK","ON  2,5-M10",null,"Oko neizolované Cu stáčené z plechu, průřez 1,5-2,5mm2 / M10 / šíře 18mm","100ks",5.2699748748380966,{"$f":"F1696*(1-Elteq!$F$9)","v":5.2699748748380966},"8591735052942"]
["TECHNIK","ON  2,5-M10/15",null,"Oko neizolované Cu stáčené z plechu, průřez 1,5-2,5mm2 / M10 / šíře 15mm","100ks",5.2699748748380966,{"$f":"F1697*(1-Elteq!$F$9)","v":5.2699748748380966},"8591735002558"]
["TECHNIK","ON  2,5-M12",null,"Oko neizolované Cu stáčené z plechu, průřez 1,5-2,5mm2 / M12 / šíře 18mm","100ks",6.6060248431069102,{"$f":"F1698*(1-Elteq!$F$9)","v":6.6060248431069102},"8591735002572"]
["TECHNIK","ON  2,5-M16",null,"Oko neizolované Cu stáčené z plechu, průřez 1,5-2,5mm2 / M16 / šíře 27mm","100ks",25.79318688741181,{"$f":"F1699*(1-Elteq!$F$9)","v":25.79318688741181},"8591735002589"]
["TECHNIK","ON  2,5-M20",null,"Oko neizolované Cu stáčené z plechu, průřez 1,5-2,5mm2 / M20 / šíře 27mm","100ks",30.024011786929719,{"$f":"F1700*(1-Elteq!$F$9)","v":30.024011786929719},"8591735033996"]
["TECHNIK","ON  6-M 3",null,"Oko neizolované Cu stáčené z plechu, průřez 4-6mm2 / M3 / šíře 7,2mm","100ks",4.861737384533737,{"$f":"F1701*(1-Elteq!$F$9)","v":4.861737384533737},"8591735002596"]
["TECHNIK","ON  6-M 3,5",null,"Oko neizolované Cu stáčené z plechu, průřez 4-6mm2 / M3,5 / šíře 8mm","100ks",4.861737384533737,{"$f":"F1702*(1-Elteq!$F$9)","v":4.861737384533737},"8591735002602"]
["TECHNIK","ON  6-M 4",null,"Oko neizolované Cu stáčené z plechu, průřez 4-6mm2 / M4 / šíře 8mm, dle DIN 46234","100ks",4.6761748889408468,{"$f":"F1703*(1-Elteq!$F$9)","v":4.6761748889408468},"8591735002619"]
["TECHNIK","ON  6-M 5",null,"Oko neizolované Cu stáčené z plechu, průřez 4-6mm2 / M5 / šíře 10mm, dle DIN 46234","100ks",5.0844123792452063,{"$f":"F1704*(1-Elteq!$F$9)","v":5.0844123792452063},"8591735002626"]
["TECHNIK","ON  6-M 6",null,"Oko neizolované Cu stáčené z plechu, průřez 4-6mm2 / M6 / šíře 11mm, dle DIN 46234","100ks",5.5297623686681439,{"$f":"F1705*(1-Elteq!$F$9)","v":5.5297623686681439},"8591735002633"]
["TECHNIK","ON  6-M 8",null,"Oko neizolované Cu stáčené z plechu, průřez 4-6mm2 / M8 / šíře 14mm, dle DIN 46234","100ks",7.0142623334112697,{"$f":"F1706*(1-Elteq!$F$9)","v":7.0142623334112697},"8591735002640"]
["TECHNIK","ON  6-M10",null,"Oko neizolované Cu stáčené z plechu, průřez 4-6mm2 / M10 / šíře 18mm, dle DIN 46234","100ks",8.7214372928658648,{"$f":"F1707*(1-Elteq!$F$9)","v":8.7214372928658648},"8591735002657"]
["TECHNIK","ON  6-M12",null,"Oko neizolované Cu stáčené z plechu, průřez 4-6mm2 / M12 / šíře 18mm","100ks",9.0554497849330673,{"$f":"F1708*(1-Elteq!$F$9)","v":9.0554497849330673},"8591735002671"]
["TECHNIK","ON  6-M16",null,"Oko neizolované Cu stáčené z plechu, průřez 4-6mm2 / M16 / šíře 24mm","100ks",21.896374479961107,{"$f":"F1709*(1-Elteq!$F$9)","v":21.896374479961107},"8591735002688"]
["TECHNIK","ON  6-M16/32",null,"Oko neizolované Cu stáčené z plechu, průřez 4-6mm2 / M16 / šíře 32mm","100ks",28.762186816898062,{"$f":"F1710*(1-Elteq!$F$9)","v":28.762186816898062},"8591735035556"]
["TECHNIK","ON  6-M20",null,"Oko neizolované Cu stáčené z plechu, průřez 4-6mm2 / M20 / šíře 32mm","100ks",34.997086668819193,{"$f":"F1711*(1-Elteq!$F$9)","v":34.997086668819193},"8591735034009"]
["TECHNIK","ON 10-M 4",null,"Oko neizolované Cu stáčené z plechu, průřez 10mm2 / M4 / šíře 10mm","100ks",10.577062248794771,{"$f":"F1712*(1-Elteq!$F$9)","v":10.577062248794771},"8591735002695"]
["TECHNIK","ON 10-M 5",null,"Oko neizolované Cu stáčené z plechu, průřez 10mm2 / M5 / šíře 10mm, dle DIN 46234","100ks",7.7936248149014107,{"$f":"F1713*(1-Elteq!$F$9)","v":7.7936248149014107},"8591735002701"]
["TECHNIK","ON 10-M 6",null,"Oko neizolované Cu stáčené z plechu, průřez 10mm2 / M6 / šíře 11mm, dle DIN 46234","100ks",8.1647498060871921,{"$f":"F1714*(1-Elteq!$F$9)","v":8.1647498060871921},"8591735002718"]
["TECHNIK","ON 10-M 8",null,"Oko neizolované Cu stáčené z plechu, průřez 10mm2 / M8 / šíře 14mm, dle DIN 46234","100ks",9.0925622840516453,{"$f":"F1715*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735002725"]
["TECHNIK","ON 10-M10",null,"Oko neizolované Cu stáčené z plechu, průřez 10mm2 / M10 / šíře 18mm, dle DIN 46234","100ks",12.247124709130787,{"$f":"F1716*(1-Elteq!$F$9)","v":12.247124709130787},"8591735002732"]
["TECHNIK","ON 10-M12",null,"Oko neizolované Cu stáčené z plechu, průřez 10mm2 / M12 / šíře 22mm, dle DIN 46234","100ks",17.44287458573173,{"$f":"F1717*(1-Elteq!$F$9)","v":17.44287458573173},"8591735002749"]
["TECHNIK","ON 10-M16",null,"Oko neizolované Cu stáčené z plechu, průřez 10mm2 / M16 / šíře 31,6mm","100ks",43.236061473143543,{"$f":"F1718*(1-Elteq!$F$9)","v":43.236061473143543},"8591735054892"]
["TECHNIK","ON 10-M20",null,"Oko neizolované Cu stáčené z plechu, průřez 10mm2 / M20 / šíře 31,6mm","100ks",51.40081127923073,{"$f":"F1719*(1-Elteq!$F$9)","v":51.40081127923073},"8591735054908"]
["TECHNIK","ON 16-M 5",null,"Oko neizolované Cu stáčené z plechu, průřez 16mm2 / M5 / šíře 11mm, dle DIN 46234","100ks",10.948187239980554,{"$f":"F1720*(1-Elteq!$F$9)","v":10.948187239980554},"8591735002756"]
["TECHNIK","ON 16-M 6",null,"Oko neizolované Cu stáčené z plechu, průřez 16mm2 / M6 / šíře 11mm, dle DIN 46234","100ks",12.80381219590946,{"$f":"F1721*(1-Elteq!$F$9)","v":12.80381219590946},"8591735002763"]
["TECHNIK","ON 16-M 8",null,"Oko neizolované Cu stáčené z plechu, průřez 16mm2 / M8 / šíře 14mm, dle DIN 46234","100ks",12.98937469150235,{"$f":"F1722*(1-Elteq!$F$9)","v":12.98937469150235},"8591735002770"]
["TECHNIK","ON 16-M10",null,"Oko neizolované Cu stáčené z plechu, průřez 16mm2 / M10 / šíře 18mm, dle DIN 46234","100ks",17.257312090138839,{"$f":"F1723*(1-Elteq!$F$9)","v":17.257312090138839},"8591735002787"]
["TECHNIK","ON 16-M12",null,"Oko neizolované Cu stáčené z plechu, průřez 16mm2 / M12 / šíře 22mm, dle DIN 46234","100ks",25.60762439181892,{"$f":"F1724*(1-Elteq!$F$9)","v":25.60762439181892},"8591735002794"]
["TECHNIK","ON 16-M16",null,"Oko neizolované Cu stáčené z plechu, průřez 16mm2 / M16 / šíře 24mm","100ks",33.215686711127439,{"$f":"F1725*(1-Elteq!$F$9)","v":33.215686711127439},"8591735015602"]
["TECHNIK","ON 16-M20",null,"Oko neizolované Cu stáčené z plechu, průřez 16mm2 / M20 / šíře 31,6mm","100ks",58.823311102946363,{"$f":"F1726*(1-Elteq!$F$9)","v":58.823311102946363},"8591735054915"]
["TECHNIK","ON 25-M 5",null,"Oko neizolované Cu stáčené z plechu, průřez 25mm2 / M5 / šíře 12mm, dle DIN 46234","100ks",21.896374479961107,{"$f":"F1727*(1-Elteq!$F$9)","v":21.896374479961107},"8591735010201"]
["TECHNIK","ON 25-M 6",null,"Oko neizolované Cu stáčené z plechu, průřez 25mm2 / M6 / šíře 12mm, dle DIN 46234","100ks",23.751999435890014,{"$f":"F1728*(1-Elteq!$F$9)","v":23.751999435890014},"8591735010218"]
["TECHNIK","ON 25-M 8",null,"Oko neizolované Cu stáčené z plechu, průřez 25mm2 / M8 / šíře 16mm, dle DIN 46234","100ks",23.195311949111343,{"$f":"F1729*(1-Elteq!$F$9)","v":23.195311949111343},"8591735002800"]
["TECHNIK","ON 25-M10",null,"Oko neizolované Cu stáčené z plechu, průřez 25mm2 / M10 / šíře 18mm, dle DIN 46234","100ks",27.092124356562046,{"$f":"F1730*(1-Elteq!$F$9)","v":27.092124356562046},"8591735010225"]
["TECHNIK","ON 25-M12",null,"Oko neizolované Cu stáčené z plechu, průřez 25mm2 / M12 / šíře 22mm, dle DIN 46234","100ks",33.77237419790611,{"$f":"F1731*(1-Elteq!$F$9)","v":33.77237419790611},"8591735010232"]
["TECHNIK","ON 25-M16",null,"Oko neizolované Cu stáčené z plechu, průřez 25mm2 / M16 / šíře 28mm, dle DIN 46234","100ks",46.390623898222685,{"$f":"F1732*(1-Elteq!$F$9)","v":46.390623898222685},"8591735010249"]
["TECHNIK","ON 25-M20",null,"Oko neizolované Cu stáčené z plechu, průřez 25mm2 / M20 / šíře 30mm","100ks",69.771498342926918,{"$f":"F1733*(1-Elteq!$F$9)","v":69.771498342926918},"8591735054922"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"ON 35-M 6",null,"Oko neizolované Cu stáčené z plechu, průřez 35mm2 / M6 / šíře 15mm, dle DIN 46234","100ks",28.576624321305172,{"$f":"F1734*(1-Elteq!$F$9)","v":28.576624321305172},"8591735002817"]
["TECHNIK","ON 35-M 8",null,"Oko neizolované Cu stáčené z plechu, průřez 35mm2 / M8 / šíře 16mm, dle DIN 46234","100ks",28.576624321305172,{"$f":"F1735*(1-Elteq!$F$9)","v":28.576624321305172},"8591735002824"]
["TECHNIK","ON 35-M10",null,"Oko neizolované Cu stáčené z plechu, průřez 35mm2 / M10 / šíře 18mm, dle DIN 46234","100ks",33.215686711127439,{"$f":"F1736*(1-Elteq!$F$9)","v":33.215686711127439},"8591735010256"]
["TECHNIK","ON 35-M12",null,"Oko neizolované Cu stáčené z plechu, průřez 35mm2 / M12 / šíře 22mm, dle DIN 46234","100ks",38.968124074507053,{"$f":"F1737*(1-Elteq!$F$9)","v":38.968124074507053},"8591735010263"]
["TECHNIK","ON 35-M16",null,"Oko neizolované Cu stáčené z plechu, průřez 35mm2 / M16 / šíře 28mm, dle DIN 46234","100ks",53.813123721938311,{"$f":"F1738*(1-Elteq!$F$9)","v":53.813123721938311},"8591735010270"]
["TECHNIK","ON 35-M20",null,"Oko neizolované Cu stáčené z plechu, průřez 35mm2 / M20 / šíře 30mm","100ks",101.68824758490412,{"$f":"F1739*(1-Elteq!$F$9)","v":101.68824758490412},"8591735031282"]
["TECHNIK","ON 50-M 6",null,"Oko neizolované Cu stáčené z plechu, průřez 50mm2 / M6 / šíře 18mm, dle DIN 46234","50ks",23.009749453518449,{"$f":"F1740*(1-Elteq!$F$9)","v":23.009749453518449},"8591735002831"]
["TECHNIK","ON 50-M 8",null,"Oko neizolované Cu stáčené z plechu, průřez 50mm2 / M8 / šíře 18mm, dle DIN 46234","50ks",23.009749453518449,{"$f":"F1741*(1-Elteq!$F$9)","v":23.009749453518449},"8591735002848"]
["TECHNIK","ON 50-M10",null,"Oko neizolované Cu stáčené z plechu, průřez 50mm2 / M10 / šíře 18mm, dle DIN 46234","50ks",23.751999435890014,{"$f":"F1742*(1-Elteq!$F$9)","v":23.751999435890014},"8591735002855"]
["TECHNIK","ON 50-M12",null,"Oko neizolované Cu stáčené z plechu, průřez 50mm2 / M12 / šíře 22mm, dle DIN 46234","50ks",30.617811772826972,{"$f":"F1743*(1-Elteq!$F$9)","v":30.617811772826972},"8591735010287"]
["TECHNIK","ON 50-M16",null,"Oko neizolované Cu stáčené z plechu, průřez 50mm2 / M16 / šíře 28mm, dle DIN 46234","50ks",41.009311526028853,{"$f":"F1744*(1-Elteq!$F$9)","v":41.009311526028853},"8591735010294"]
["TECHNIK","ON 50-M20",null,"Oko neizolované Cu stáčené z plechu, průřez 50mm2 / M20 / šíře 32mm","50ks",52.514186252788079,{"$f":"F1745*(1-Elteq!$F$9)","v":52.514186252788079},"8591735054793"]
["TECHNIK","ON 70-M 6",null,"Oko neizolované Cu stáčené z plechu, průřez 70mm2 / M6 / šíře 22mm, dle DIN 46234","50ks",33.77237419790611,{"$f":"F1746*(1-Elteq!$F$9)","v":33.77237419790611},"8591735010300"]
["TECHNIK","ON 70-M 8",null,"Oko neizolované Cu stáčené z plechu, průřez 70mm2 / M8 / šíře 22mm, dle DIN 46234","50ks",33.77237419790611,{"$f":"F1747*(1-Elteq!$F$9)","v":33.77237419790611},"8591735010317"]
["TECHNIK","ON 70-M10",null,"Oko neizolované Cu stáčené z plechu, průřez 70mm2 / M10 / šíře 22mm, dle DIN 46234","50ks",40.823749030435962,{"$f":"F1748*(1-Elteq!$F$9)","v":40.823749030435962},"8591735010324"]
["TECHNIK","ON 70-M12",null,"Oko neizolované Cu stáčené z plechu, průřez 70mm2 / M12 / šíře 22mm, dle DIN 46234","50ks",33.77237419790611,{"$f":"F1749*(1-Elteq!$F$9)","v":33.77237419790611},"8591735010331"]
["TECHNIK","ON 70-M16",null,"Oko neizolované Cu stáčené z plechu, průřez 70mm2 / M16 / šíře 28mm, dle DIN 46234","50ks",55.668748677867221,{"$f":"F1750*(1-Elteq!$F$9)","v":55.668748677867221},"8591735010348"]
["TECHNIK","ON 70-M20",null,"Oko neizolované Cu stáčené z plechu, průřez 70mm2 / M20 / šíře 32mm","25ks",31.545624250791423,{"$f":"F1751*(1-Elteq!$F$9)","v":31.545624250791423},"8591735054809"]
["TECHNIK","ON 95-M 8",null,"Oko neizolované Cu stáčené z plechu, průřez 95mm2 / M8 / šíře 24mm, dle DIN 46234","25ks",34.700186675870569,{"$f":"F1752*(1-Elteq!$F$9)","v":34.700186675870569},"8591735010355"]
["TECHNIK","ON 95-M10",null,"Oko neizolované Cu stáčené z plechu, průřez 95mm2 / M10 / šíře 24mm, dle DIN 46234","25ks",30.803374268419862,{"$f":"F1753*(1-Elteq!$F$9)","v":30.803374268419862},"8591735002862"]
["TECHNIK","ON 95-M12",null,"Oko neizolované Cu stáčené z plechu, průřez 95mm2 / M12 / šíře 24mm, dle DIN 46234","25ks",30.803374268419862,{"$f":"F1754*(1-Elteq!$F$9)","v":30.803374268419862},"8591735002879"]
["TECHNIK","ON 95-M16",null,"Oko neizolované Cu stáčené z plechu, průřez 95mm2 / M16 / šíře 28mm, dle DIN 46234","25ks",38.040311596542601,{"$f":"F1755*(1-Elteq!$F$9)","v":38.040311596542601},"8591735010362"]
["TECHNIK","ON120-M 8",null,"Oko neizolované Cu stáčené z plechu, průřez 120mm2 / M8 / šíře 24mm, dle DIN 46234","25ks",51.40081127923073,{"$f":"F1756*(1-Elteq!$F$9)","v":51.40081127923073},"8591735002886"]
["TECHNIK","ON120-M10",null,"Oko neizolované Cu stáčené z plechu, průřez 120mm2 / M10 / šíře 24mm, dle DIN 46234","25ks",50.101873810080498,{"$f":"F1757*(1-Elteq!$F$9)","v":50.101873810080498},"8591735002893"]
["TECHNIK","ON120-M12",null,"Oko neizolované Cu stáčené z plechu, průřez 120mm2 / M12 / šíře 24mm, dle DIN 46234","25ks",52.143061261602298,{"$f":"F1758*(1-Elteq!$F$9)","v":52.143061261602298},"8591735010379"]
["TECHNIK","ON120-M16",null,"Oko neizolované Cu stáčené z plechu, průřez 120mm2 / M16 / šíře 28mm, dle DIN 46234","25ks",69.585935847334028,{"$f":"F1759*(1-Elteq!$F$9)","v":69.585935847334028},"8591735016302"]
["TECHNIK","ON120-M20",null,"Oko neizolované Cu stáčené z plechu, průřez 120mm2 / M20 / šíře 32mm, dle DIN 46234","25ks",71.998248290041602,{"$f":"F1760*(1-Elteq!$F$9)","v":71.998248290041602},"8591735031299"]
["TECHNIK","ON150-M10",null,"Oko neizolované Cu stáčené z plechu, průřez 150mm2 / M10 / šíře 30mm, dle DIN 46234","25ks",74.410560732749175,{"$f":"F1761*(1-Elteq!$F$9)","v":74.410560732749175},"8591735010386"]
["TECHNIK","ON150-M12",null,"Oko neizolované Cu stáčené z plechu, průřez 150mm2 / M12 / šíře 30mm, dle DIN 46234","25ks",88.142185406623099,{"$f":"F1762*(1-Elteq!$F$9)","v":88.142185406623099},"8591735010393"]
["TECHNIK","ON150-M16",null,"Oko neizolované Cu stáčené z plechu, průřez 150mm2 / M16 / šíře 30mm, dle DIN 46234","25ks",103.9149975320188,{"$f":"F1763*(1-Elteq!$F$9)","v":103.9149975320188},"8591735010409"]
["TECHNIK","ON185-M10",null,"Oko neizolované Cu stáčené z plechu, průřez 185mm2 / M10 / šíře 36mm, dle DIN 46234","25ks",93.709060274409822,{"$f":"F1764*(1-Elteq!$F$9)","v":93.709060274409822},"8591735018399"]
["TECHNIK","ON185-M12",null,"Oko neizolované Cu stáčené z plechu, průřez 185mm2 / M12 / šíře 36mm, dle DIN 46234","25ks",93.709060274409822,{"$f":"F1765*(1-Elteq!$F$9)","v":93.709060274409822},"8591735010416"]
["TECHNIK","ON185-M16",null,"Oko neizolované Cu stáčené z plechu, průřez 185mm2 / M16 / šíře 36mm, dle DIN 46234","25ks",92.224560309666685,{"$f":"F1766*(1-Elteq!$F$9)","v":92.224560309666685},"8591735010423"]
["TECHNIK","ON240-M10",null,"Oko neizolované Cu stáčené z plechu, průřez 240mm2 / M10 / šíře 38mm, dle DIN 46234","25ks",120.61562213537897,{"$f":"F1767*(1-Elteq!$F$9)","v":120.61562213537897},"8591735031305"]
["TECHNIK","ON240-M12",null,"Oko neizolované Cu stáčené z plechu, průřez 240mm2 / M12 / šíře 38mm, dle DIN 46234","25ks",120.61562213537897,{"$f":"F1768*(1-Elteq!$F$9)","v":120.61562213537897},"8591735010447"]
["TECHNIK","ON240-M16",null,"Oko neizolované Cu stáčené z plechu, průřez 240mm2 / M16 / šíře 38mm, dle DIN 46234","25ks",134.53280930484578,{"$f":"F1769*(1-Elteq!$F$9)","v":134.53280930484578},"8591735010430"]
["TECHNIK","ON300-M12",null,"Oko neizolované Cu stáčené z plechu, průřez 300mm2 / M12 / šíře 30mm","15ks",158.84149622751445,{"$f":"F1770*(1-Elteq!$F$9)","v":158.84149622751445},"8591735027056"]
["TECHNIK","ONM 1,5-M 3",null,"Oko neizolované mosazné mechanicky odolné, průřez 0,5-1,5mm2 / M3 / šíře 7mm, dle DIN 46225","100ks",2.4494249418261576,{"$f":"F1771*(1-Elteq!$F$9)","v":2.4494249418261576},"8591735007553"]
["TECHNIK","ONM 1,5-M 4",null,"Oko neizolované mosazné mechanicky odolné, průřez 0,5-1,5mm2 / M4 / šíře 7mm","100ks",2.5978749383004702,{"$f":"F1772*(1-Elteq!$F$9)","v":2.5978749383004702},"8591735007560"]
["TECHNIK","ONM 1,5-M 4/9",null,"Oko neizolované mosazné mechanicky odolné, průřez 0,5-1,5mm2 / M4 / šíře 8,7mm","100ks",3.0803374268419863,{"$f":"F1773*(1-Elteq!$F$9)","v":3.0803374268419863},"8591735023935"]
["TECHNIK","ONM 1,5-M 5",null,"Oko neizolované mosazné mechanicky odolné, průřez 0,5-1,5mm2 / M5 / šíře 11mm","100ks",3.0803374268419863,{"$f":"F1774*(1-Elteq!$F$9)","v":3.0803374268419863},"8591735007577"]
["TECHNIK","ONM 1,5-M 5/9",null,"Oko neizolované mosazné mechanicky odolné, průřez 0,5-1,5mm2 / M5 / šíře 9,5mm","100ks",5.9379998589725034,{"$f":"F1775*(1-Elteq!$F$9)","v":5.9379998589725034},"8591735033248"]
["TECHNIK","ONM 1,5-M 6",null,"Oko neizolované mosazné mechanicky odolné, průřez 0,5-1,5mm2 / M6 / šíře 9mm","100ks",5.9008873598539253,{"$f":"F1776*(1-Elteq!$F$9)","v":5.9008873598539253},"8591735015756"]
["TECHNIK","ONM 1,5-M 6/12",null,"Oko neizolované mosazné mechanicky odolné, průřez 0,5-1,5mm2 / M6 / 12mm","100ks",8.0162998096128799,{"$f":"F1777*(1-Elteq!$F$9)","v":8.0162998096128799},"8591735031312"]
["TECHNIK","ONM 1,5-M 8",null,"Oko neizolované mosazné mechanicky odolné, průřez 0,5-1,5mm2 / M8 / 14mm","100ks",7.6451748184270985,{"$f":"F1778*(1-Elteq!$F$9)","v":7.6451748184270985},"8591735025533"]
["TECHNIK","ONM 1,5-M10",null,"Oko neizolované mosazné mechanicky odolné, průřez 0,5-1,5mm2 / M10 / 18,5mm","100ks",8.869887289340177,{"$f":"F1779*(1-Elteq!$F$9)","v":8.869887289340177},"8591735025540"]
["TECHNIK","ONM 2,5-M 4",null,"Oko neizolované mosazné mechanicky odolné, průřez 1,0-2,5mm2 / M4 / 8,7mm","100ks",3.1916749241977205,{"$f":"F1780*(1-Elteq!$F$9)","v":3.1916749241977205},"8591735007584"]
["TECHNIK","ONM 2,5-M 5",null,"Oko neizolované mosazné mechanicky odolné, průřez 1,0-2,5mm2 / M5 / 8,7mm","100ks",3.1916749241977205,{"$f":"F1781*(1-Elteq!$F$9)","v":3.1916749241977205},"8591735007591"]
["TECHNIK","ONM 2,5-M 6",null,"Oko neizolované mosazné mechanicky odolné, průřez 1,0-2,5mm2 / M6 / 9mm","100ks",3.1916749241977205,{"$f":"F1782*(1-Elteq!$F$9)","v":3.1916749241977205},"8591735007607"]
["TECHNIK","ONM 2,5-M 6/12",null,"Oko neizolované mosazné mechanicky odolné, průřez 1,0-2,5mm2 / M6 / 12mm","100ks",5.4555373704309877,{"$f":"F1783*(1-Elteq!$F$9)","v":5.4555373704309877},"8591735023942"]
["TECHNIK","ONM 2,5-M 8",null,"Oko neizolované mosazné mechanicky odolné, průřez 1,5-2,5mm2 / M8 / 12mm","100ks",8.6100997955101306,{"$f":"F1784*(1-Elteq!$F$9)","v":8.6100997955101306},"8591735023959"]
["TECHNIK","ONM 2,5-M10",null,"Oko neizolované mosazné mechanicky odolné, průřez 1,5-2,5mm2 / M10 / 18mm","100ks",10.948187239980554,{"$f":"F1785*(1-Elteq!$F$9)","v":10.948187239980554},"8591735021313"]
["TECHNIK","ONM 4-M 6",null,"Oko neizolované mosazné mechanicky odolné, průřez 3-6mm2 / M6 / šíře 12mm / délka 19mm","100ks",5.0472998801266282,{"$f":"F1786*(1-Elteq!$F$9)","v":5.0472998801266282},"8591735007614"]
["TECHNIK","ONM 4-M 7",null,"Oko neizolované mosazné mechanicky odolné, průřez 3-6mm2 / M7 / šíře 12mm / délka 19mm","100ks",5.0472998801266282,{"$f":"F1787*(1-Elteq!$F$9)","v":5.0472998801266282},"8591735007621"]
["TECHNIK","ONM 4-M 8",null,"Oko neizolované mosazné mechanicky odolné, průřez 3-6mm2 / M8 / šíře 13,7mm / délka 20mm","100ks",5.0472998801266282,{"$f":"F1788*(1-Elteq!$F$9)","v":5.0472998801266282},"8591735007638"]
["TECHNIK","ONM 4-M 8/14",null,"Oko neizolované mosazné mechanicky odolné, průřez 3-6mm2 / M8 / šíře 14mm / délka 31mm","100ks",7.0142623334112697,{"$f":"F1789*(1-Elteq!$F$9)","v":7.0142623334112697},""]
["TECHNIK","ONM 4-M10",null,"Oko neizolované mosazné mechanicky odolné, průřez 3-6mm2 / M10 / šíře 16mm / délka 32mm","100ks",7.7193998166642546,{"$f":"F1790*(1-Elteq!$F$9)","v":7.7193998166642546},"8591735007645"]
["TECHNIK","ONM 6-M 4",null,"Oko neizolované mosazné mechanicky odolné, průřez 4-6mm2 / M4 / šíře 8mm","100ks",8.090524807850036,{"$f":"F1791*(1-Elteq!$F$9)","v":8.090524807850036},"8591735021559"]
["TECHNIK","ONMC 1,5-M 3",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 0,5-1,5mm2 / M3 / šíře 7mm","100ks",3.0803374268419863,{"$f":"F1792*(1-Elteq!$F$9)","v":3.0803374268419863},"8591735023966"]
["TECHNIK","ONMC 1,5-M 3/9",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 0,5-1,5mm2 / M3 / 8,7mm","100ks",3.3030124215534551,{"$f":"F1793*(1-Elteq!$F$9)","v":3.3030124215534551},"8591735023973"]
["TECHNIK","ONMC 1,5-M 4",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 0,5-1,5mm2 / M4 / 7mm","100ks",2.783437433893361,{"$f":"F1794*(1-Elteq!$F$9)","v":2.783437433893361},"8591735015763"]
["TECHNIK","ONMC 1,5-M 4/9",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 0,5-1,5mm2 / M4 / 8,7mm","100ks",3.3030124215534551,{"$f":"F1795*(1-Elteq!$F$9)","v":3.3030124215534551},"8591735023980"]
["TECHNIK","ONMC 1,5-M 5",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 0,5-1,5mm2 / M5 / 11mm","100ks",3.4885749171463458,{"$f":"F1796*(1-Elteq!$F$9)","v":3.4885749171463458},"8591735024611"]
["TECHNIK","ONMC 1,5-M 5/9",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 0,5-1,5mm2 / M5 / 8,7mm","100ks",3.3030124215534551,{"$f":"F1797*(1-Elteq!$F$9)","v":3.3030124215534551},"8591735023997"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"ONMC 1,5-M 6",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 0,5-1,5mm2 / M6 / šíře 8,7mm","100ks",4.00814990480644,{"$f":"F1798*(1-Elteq!$F$9)","v":4.00814990480644},"8591735024000"]
["TECHNIK","ONMC 1,5-M 6/12",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 1,0-1,5mm2 / M6 / 12mm","100ks",9.8719247655417863,{"$f":"F1799*(1-Elteq!$F$9)","v":9.8719247655417863},"8591735024017"]
["TECHNIK","ONMC 1,5-M 8",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 1,0-1,5mm2 / M8 / 14mm","100ks",8.6472122946287087,{"$f":"F1800*(1-Elteq!$F$9)","v":8.6472122946287087},"8591735021078"]
["TECHNIK","ONMC 2,5-M 3",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 1,5-2,5mm2 / M3 / šíře 8mm","100ks",8.6472122946287087,{"$f":"F1801*(1-Elteq!$F$9)","v":8.6472122946287087},"8591735021306"]
["TECHNIK","ONMC 2,5-M 4",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 1,0-2,5mm2 / M4 / 8,7mm","100ks",3.9339249065692834,{"$f":"F1802*(1-Elteq!$F$9)","v":3.9339249065692834},"8591735024024"]
["TECHNIK","ONMC 2,5-M 5",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 1,5-2,5mm2 / M5 / 8,7mm","100ks",4.1565999012807522,{"$f":"F1803*(1-Elteq!$F$9)","v":4.1565999012807522},"8591735024031"]
["TECHNIK","ONMC 2,5-M 5/9",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 1,5-2,5mm2 / M5 / 9,5mm","100ks",6.420462347514019,{"$f":"F1804*(1-Elteq!$F$9)","v":6.420462347514019},"8591735021146"]
["TECHNIK","ONMC 2,5-M 6",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 1,5-2,5mm2 / M6 / šíře 8,7mm","100ks",4.1565999012807522,{"$f":"F1805*(1-Elteq!$F$9)","v":4.1565999012807522},"8591735024048"]
["TECHNIK","ONMC 2,5-M 6/12",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 1,5-2,5mm2 / M6 / 12mm","100ks",8.6472122946287087,{"$f":"F1806*(1-Elteq!$F$9)","v":8.6472122946287087},"8591735021542"]
["TECHNIK","ONMC 2,5-M 8",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 1,5-2,5mm2 / M8 / 14mm / délka 28mm","100ks",9.7234747690674741,{"$f":"F1807*(1-Elteq!$F$9)","v":9.7234747690674741},"8591735024055"]
["TECHNIK","ONMC 2,5-M 8/1",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 1,5-2,5mm2 / M8 / 14mm / délka 28mm","100ks",9.7234747690674741,{"$f":"F1808*(1-Elteq!$F$9)","v":9.7234747690674741},"8591735021177"]
["TECHNIK","ONMC 2,5-M10",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 1,5-2,5mm2 / M10 / 18mm","100ks",12.61824970031657,{"$f":"F1809*(1-Elteq!$F$9)","v":12.61824970031657},"8591735055400"]
["TECHNIK","ONMC 2,5-M12",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 1,5-2,5mm2 / M12 / 18mm","100ks",17.44287458573173,{"$f":"F1810*(1-Elteq!$F$9)","v":17.44287458573173},"8591735021283"]
["TECHNIK","ONMC 4-M 6",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 3-6mm2 / M6 / šíře 12mm / délka 19mm","100ks",5.641099866023878,{"$f":"F1811*(1-Elteq!$F$9)","v":5.641099866023878},"8591735055219"]
["TECHNIK","ONMC 4-M 7",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 3-6mm2 / M7 / šíře 12mm / délka 19mm","100ks",6.1977873528025507,{"$f":"F1812*(1-Elteq!$F$9)","v":6.1977873528025507},"8591735033415"]
["TECHNIK","ONMC 4-M 8",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 3-6mm2 / M8 / šíře 13,7mm / délka 20mm","100ks",6.1977873528025507,{"$f":"F1813*(1-Elteq!$F$9)","v":6.1977873528025507},"8591735031329"]
["TECHNIK","ONMC 4-M 8/14",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 3-6mm2 / M8 / šíře 14mm / délka 31mm","100ks",7.6080623193085195,{"$f":"F1814*(1-Elteq!$F$9)","v":7.6080623193085195},""]
["TECHNIK","ONMC 4-M10",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 3-6mm2 / M10 / šíře 16mm / délka 32mm","100ks",10.577062248794771,{"$f":"F1815*(1-Elteq!$F$9)","v":10.577062248794771},"8591735024086"]
["TECHNIK","ONMC 6-M 4",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 4-6mm2 / M4 / 8mm","100ks",11.690437222352116,{"$f":"F1816*(1-Elteq!$F$9)","v":11.690437222352116},"8591735021184"]
["TECHNIK","ONMC 6-M 5",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 4-6mm2 / M5 / 9,5mm","100ks",10.911074740861975,{"$f":"F1817*(1-Elteq!$F$9)","v":10.911074740861975},"8591735021290"]
["TECHNIK","ONMC 6-M 6",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 4-6mm2 / M6 / 12mm","100ks",10.911074740861975,{"$f":"F1818*(1-Elteq!$F$9)","v":10.911074740861975},"8591735024062"]
["TECHNIK","ONMC 6-M 8",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 4-6mm2 / M8 / 14mm","100ks",11.096637236454866,{"$f":"F1819*(1-Elteq!$F$9)","v":11.096637236454866},"8591735024079"]
["TECHNIK","ONMC10-M 5",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 6-10mm2 / M5","100ks",20.597437010810872,{"$f":"F1820*(1-Elteq!$F$9)","v":20.597437010810872},"8591735031336"]
["TECHNIK","ONMC10-M 6",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 6-10mm2 / M6","100ks",17.183087091901683,{"$f":"F1821*(1-Elteq!$F$9)","v":17.183087091901683},"8591735031343"]
["TECHNIK","ONMC10-M 8",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 6-10mm2 / M8","100ks",17.183087091901683,{"$f":"F1822*(1-Elteq!$F$9)","v":17.183087091901683},"8591735031350"]
["TECHNIK","ONMC10-M10",null,"Oko neizolované mosazné cínované mechanicky odolné, průřez 6-10mm2 / M10","100ks",21.896374479961107,{"$f":"F1823*(1-Elteq!$F$9)","v":21.896374479961107},"8591735031367"]
["TECHNIK","OIS 1,5-M 2,5",null,"Oko lisovací se smršťovací bužírkou, průřez 0,5-1,5mm2 / M2,5 / 6mm","100ks",13.917187169466805,{"$f":"F1824*(1-Elteq!$F$9)","v":13.917187169466805},"8591735031107"]
["TECHNIK","OIS 1,5-M 3",null,"Oko lisovací se smršťovací bužírkou, průřez 0,5-1,5mm2 / M3 / 6mm","100ks",13.917187169466805,{"$f":"F1825*(1-Elteq!$F$9)","v":13.917187169466805},"8591735024345"]
["TECHNIK","OIS 1,5-M 3,5",null,"Oko lisovací se smršťovací bužírkou, průřez 0,5-1,5mm2 / M3,5 / 6,6mm","100ks",13.917187169466805,{"$f":"F1826*(1-Elteq!$F$9)","v":13.917187169466805},"8591735031114"]
["TECHNIK","OIS 1,5-M 4",null,"Oko lisovací se smršťovací bužírkou, průřez 0,5-1,5mm2 / M4 / 8mm","100ks",13.917187169466805,{"$f":"F1827*(1-Elteq!$F$9)","v":13.917187169466805},"8591735024352"]
["TECHNIK","OIS 1,5-M 4/7",null,"Oko lisovací se smršťovací bužírkou, průřez 0,5-1,5mm2 / M4 / 6,8mm","100ks",13.917187169466805,{"$f":"F1828*(1-Elteq!$F$9)","v":13.917187169466805},"8591735031121"]
["TECHNIK","OIS 1,5-M 5",null,"Oko lisovací se smršťovací bužírkou, průřez 0,5-1,5mm2 / M5 / 10mm","100ks",13.917187169466805,{"$f":"F1829*(1-Elteq!$F$9)","v":13.917187169466805},"8591735024369"]
["TECHNIK","OIS 1,5-M 5/8",null,"Oko lisovací se smršťovací bužírkou, průřez 0,5-1,5mm2 / M5 / 8mm","100ks",13.917187169466805,{"$f":"F1830*(1-Elteq!$F$9)","v":13.917187169466805},"8591735031138"]
["TECHNIK","OIS 1,5-M 6",null,"Oko lisovací se smršťovací bužírkou, průřez 0,5-1,5mm2 / M6 / 11mm","100ks",15.401687134209931,{"$f":"F1831*(1-Elteq!$F$9)","v":15.401687134209931},"8591735024376"]
["TECHNIK","OIS 1,5-M 8",null,"Oko lisovací se smršťovací bužírkou, průřez 0,5-1,5mm2 / M8 / 14mm","100ks",15.401687134209931,{"$f":"F1832*(1-Elteq!$F$9)","v":15.401687134209931},"8591735024383"]
["TECHNIK","OIS 1,5-M 8/12",null,"Oko lisovací se smršťovací bužírkou, průřez 0,5-1,5mm2 / M8 / 12mm","100ks",15.401687134209931,{"$f":"F1833*(1-Elteq!$F$9)","v":15.401687134209931},"8591735031145"]
["TECHNIK","OIS 1,5-M10",null,"Oko lisovací se smršťovací bužírkou, průřez 0,5-1,5mm2 / M10 / 18mm","100ks",15.958374620988602,{"$f":"F1834*(1-Elteq!$F$9)","v":15.958374620988602},"8591735024390"]
["TECHNIK","OIS 1,5-M10/15",null,"Oko lisovací se smršťovací bužírkou, průřez 0,5-1,5mm2 / M10 / 14,5mm","100ks",15.958374620988602,{"$f":"F1835*(1-Elteq!$F$9)","v":15.958374620988602},"8591735031152"]
["TECHNIK","OIS 2,5-M 3",null,"Oko lisovací se smršťovací bužírkou, průřez 1,5-2,5mm2 / M3 / 6mm","100ks",14.473874656245476,{"$f":"F1836*(1-Elteq!$F$9)","v":14.473874656245476},"8591735031169"]
["TECHNIK","OIS 2,5-M 3,5",null,"Oko lisovací se smršťovací bužírkou, průřez 1,5-2,5mm2 / M3,5 / 6,6mm","100ks",14.473874656245476,{"$f":"F1837*(1-Elteq!$F$9)","v":14.473874656245476},"8591735031176"]
["TECHNIK","OIS 2,5-M 4",null,"Oko lisovací se smršťovací bužírkou, průřez 1,5-2,5mm2 / M4 / 8mm","100ks",14.473874656245476,{"$f":"F1838*(1-Elteq!$F$9)","v":14.473874656245476},"8591735024406"]
["TECHNIK","OIS 2,5-M 4/7",null,"Oko lisovací se smršťovací bužírkou, průřez 1,5-2,5mm2 / M4 / 6,8mm","100ks",14.473874656245476,{"$f":"F1839*(1-Elteq!$F$9)","v":14.473874656245476},"8591735031183"]
["TECHNIK","OIS 2,5-M 5",null,"Oko lisovací se smršťovací bužírkou, průřez 1,5-2,5mm2 / M5 / 10mm","100ks",14.473874656245476,{"$f":"F1840*(1-Elteq!$F$9)","v":14.473874656245476},"8591735024413"]
["TECHNIK","OIS 2,5-M 5/8",null,"Oko lisovací se smršťovací bužírkou, průřez 1,5-2,5mm2 / M5 / 8mm","100ks",14.473874656245476,{"$f":"F1841*(1-Elteq!$F$9)","v":14.473874656245476},"8591735031190"]
["TECHNIK","OIS 2,5-M 6",null,"Oko lisovací se smršťovací bužírkou, průřez 1,5-2,5mm2 / M6 / 11mm","100ks",15.216124638617039,{"$f":"F1842*(1-Elteq!$F$9)","v":15.216124638617039},"8591735024420"]
["TECHNIK","OIS 2,5-M 8",null,"Oko lisovací se smršťovací bužírkou, průřez 1,5-2,5mm2 / M8 / 14mm","100ks",15.216124638617039,{"$f":"F1843*(1-Elteq!$F$9)","v":15.216124638617039},"8591735024437"]
["TECHNIK","OIS 2,5-M 8/12",null,"Oko lisovací se smršťovací bužírkou, průřez 1,5-2,5mm2 / M8 / 12mm","100ks",15.216124638617039,{"$f":"F1844*(1-Elteq!$F$9)","v":15.216124638617039},"8591735031206"]
["TECHNIK","OIS 2,5-M10",null,"Oko lisovací se smršťovací bužírkou, průřez 1,5-2,5mm2 / M10 / 18mm","100ks",16.329499612174384,{"$f":"F1845*(1-Elteq!$F$9)","v":16.329499612174384},"8591735024444"]
["TECHNIK","OIS 2,5-M10/15",null,"Oko lisovací se smršťovací bužírkou, průřez 1,5-2,5mm2 / M10 / 15mm","100ks",16.329499612174384,{"$f":"F1846*(1-Elteq!$F$9)","v":16.329499612174384},"8591735031213"]
["TECHNIK","OIS 2,5-M12",null,"Oko lisovací se smršťovací bužírkou, průřez 1,5-2,5mm2 / M12 / 18mm","100ks",18.185124568103291,{"$f":"F1847*(1-Elteq!$F$9)","v":18.185124568103291},"8591735031220"]
["TECHNIK","OIS 6-M 3",null,"Oko lisovací se smršťovací bužírkou, průřez 4-6mm2 / M3 / 7,2mm","100ks",20.597437010810872,{"$f":"F1848*(1-Elteq!$F$9)","v":20.597437010810872},"8591735031237"]
["TECHNIK","OIS 6-M 3,5",null,"Oko lisovací se smršťovací bužírkou, průřez 4-6mm2 / M3,5 / 7,2mm","100ks",20.597437010810872,{"$f":"F1849*(1-Elteq!$F$9)","v":20.597437010810872},"8591735031244"]
["TECHNIK","OIS 6-M 4",null,"Oko lisovací se smršťovací bužírkou, průřez 4-6mm2 / M4 / 8mm","100ks",20.597437010810872,{"$f":"F1850*(1-Elteq!$F$9)","v":20.597437010810872},"8591735024451"]
["TECHNIK","OIS 6-M 4/10",null,"Oko lisovací se smršťovací bužírkou, průřez 4-6mm2 / M4 / 9,5mm","100ks",20.597437010810872,{"$f":"F1851*(1-Elteq!$F$9)","v":20.597437010810872},"8591735031251"]
["TECHNIK","OIS 6-M 5",null,"Oko lisovací se smršťovací bužírkou, průřez 4-6mm2 / M5 / 10mm","100ks",20.597437010810872,{"$f":"F1852*(1-Elteq!$F$9)","v":20.597437010810872},"8591735024468"]
["TECHNIK","OIS 6-M 6",null,"Oko lisovací se smršťovací bužírkou, průřez 4-6mm2 / M6 / 11mm","100ks",20.597437010810872,{"$f":"F1853*(1-Elteq!$F$9)","v":20.597437010810872},"8591735024475"]
["TECHNIK","OIS 6-M 8",null,"Oko lisovací se smršťovací bužírkou, průřez 4-6mm2 / M8 / 14mm","100ks",22.267499471146888,{"$f":"F1854*(1-Elteq!$F$9)","v":22.267499471146888},"8591735024482"]
["TECHNIK","OIS 6-M10",null,"Oko lisovací se smršťovací bužírkou, průřez 4-6mm2 / M10 / 18mm","100ks",22.267499471146888,{"$f":"F1855*(1-Elteq!$F$9)","v":22.267499471146888},"8591735024499"]
["TECHNIK","OIS 6-M10/15",null,"Oko lisovací se smršťovací bužírkou, průřez 4-6mm2 / M10 / 15mm","100ks",22.267499471146888,{"$f":"F1856*(1-Elteq!$F$9)","v":22.267499471146888},"8591735031268"]
["TECHNIK","OIS 6-M12",null,"Oko lisovací se smršťovací bužírkou, průřez 4-6mm2 / M12 / 19mm","100ks",25.60762439181892,{"$f":"F1857*(1-Elteq!$F$9)","v":25.60762439181892},"8591735031275"]
["TECHNIK","C. 1695-M10",null,"Šroubové oko cínované s trhacími šrouby na průřezy 16-95mm2 / M12, pro Al a Cu vodiče do 30kV","1ks",11.319312231166334,{"$f":"F1858*(1-Elteq!$F$9)","v":11.319312231166334},"8591735054496"]
["TECHNIK","C. 1695-M12",null,"Šroubové oko cínované s trhacími šrouby na průřezy 16-95mm2 / M12, pro Al a Cu vodiče do 30kV","1ks",11.319312231166334,{"$f":"F1859*(1-Elteq!$F$9)","v":11.319312231166334},"8591735052577"]
["TECHNIK","C. 50150-M12",null,"Šroubové oko cínované s trhacími šrouby na průřezy 50-150mm2 / M12, pro Al a Cu vodiče do 30kV","1ks",15.772812125395712,{"$f":"F1860*(1-Elteq!$F$9)","v":15.772812125395712},"8591735052584"]
["TECHNIK","C. 50150-M16",null,"Šroubové oko cínované s trhacími šrouby na průřezy 50-150mm2 / M16, pro Al a Cu vodiče do 30kV","1ks",15.772812125395712,{"$f":"F1861*(1-Elteq!$F$9)","v":15.772812125395712},"8591735052621"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"C. 95240-M12",null,"Šroubové oko cínované s trhacími šrouby na průřezy 95-240mm2 / M12, pro Al a Cu vodiče do 30kV","1ks",19.669624532846417,{"$f":"F1862*(1-Elteq!$F$9)","v":19.669624532846417},"8591735052591"]
["TECHNIK","C. 95240-M16",null,"Šroubové oko cínované s trhacími šrouby na průřezy 95-240mm2 / M16, pro Al a Cu vodiče do 30kV","1ks",19.669624532846417,{"$f":"F1863*(1-Elteq!$F$9)","v":19.669624532846417},"8591735052638"]
["TECHNIK","C.120300-M12",null,"Šroubové oko cínované s trhacími šrouby na průřezy 120-300mm2 / M12, pro Al a Cu vodiče do 30kV","1ks",29.133311808083846,{"$f":"F1864*(1-Elteq!$F$9)","v":29.133311808083846},"8591735052645"]
["TECHNIK","C.120300-M16",null,"Šroubové oko cínované s trhacími šrouby na průřezy 120-300mm2 / M16, pro Al a Cu vodiče do 30kV","1ks",29.133311808083846,{"$f":"F1865*(1-Elteq!$F$9)","v":29.133311808083846},"8591735052607"]
["TECHNIK","C.185400-M16",null,"Šroubové oko cínované s trhacími šrouby na průřezy 185-400mm2 / M16, pro Al a Cu vodiče do 30kV","1ks",34.329061684684788,{"$f":"F1866*(1-Elteq!$F$9)","v":34.329061684684788},"8591735052614"]
["TECHNIK","OLN  1,5-M4",null,"Oko lisovací z niklu do +650°C, průřez 0,5-1,5mm2 / M4 (56N4)","100ks",97.976997673046299,{"$f":"F1867*(1-Elteq!$F$9)","v":97.976997673046299},"8591735029623"]
["TECHNIK","OLN  1,5-M5",null,"Oko lisovací z niklu do +650°C, průřez 0,5-1,5mm2 / M5 (56N5)","100ks",99.832622628975216,{"$f":"F1868*(1-Elteq!$F$9)","v":99.832622628975216},"8591735029616"]
["TECHNIK","OLN  2,5-M4",null,"Oko lisovací z niklu do +650°C, průřez 1,5-2,5mm2 / M4 (57N4)","100ks",107.9973724350624,{"$f":"F1869*(1-Elteq!$F$9)","v":107.9973724350624},"8591735028718"]
["TECHNIK","OLN  2,5-M5",null,"Oko lisovací z niklu do +650°C, průřez 1,5-2,5mm2 / M5 (57N5)","100ks",114.30649728522069,{"$f":"F1870*(1-Elteq!$F$9)","v":114.30649728522069},"8591735028725"]
["TECHNIK","OLN  2,5-M6",null,"Oko lisovací z niklu do +650°C, průřez 1,5-2,5mm2 / M6 (57N6)","100ks",120.98674712656475,{"$f":"F1871*(1-Elteq!$F$9)","v":120.98674712656475},"8591735028732"]
["TECHNIK","OLN  6-M4",null,"Oko lisovací z niklu do +650°C, průřez 4-6mm2 / M4 (58N4)","100ks",145.85212153601211,{"$f":"F1872*(1-Elteq!$F$9)","v":145.85212153601211},"8591735037765"]
["TECHNIK","OLN  6-M5",null,"Oko lisovací z niklu do +650°C, průřez 4-6mm2 / M5 (58N5)","100ks",145.85212153601211,{"$f":"F1873*(1-Elteq!$F$9)","v":145.85212153601211},"8591735028749"]
["TECHNIK","OLN  6-M6",null,"Oko lisovací z niklu do +650°C, průřez 4-6mm2 / M6 (58N6)","100ks",160.32599619225758,{"$f":"F1874*(1-Elteq!$F$9)","v":160.32599619225758},"8591735029609"]
["TECHNIK","OLN 25-M8",null,"Oko lisovací z niklu do +650°C, průřez 25mm2 / M8 (61N8)","50ks",317.49742995943603,{"$f":"F1875*(1-Elteq!$F$9)","v":317.49742995943603},"8591735034016"]
["TECHNIK","OLN 50-M8",null,"Oko lisovací z niklu do +650°C, průřez 50mm2 / M8 (63N/8)","50ks",597.32567331351527,{"$f":"F1876*(1-Elteq!$F$9)","v":597.32567331351527},""]
["TECHNIK","OLN 70-M10",null,"Oko lisovací z niklu do +650°C, průřez 70mm2 / M10 (64N/10)","25ks",311.55943010046354,{"$f":"F1877*(1-Elteq!$F$9)","v":311.55943010046354},""]
["TECHNIK","OLN 95-M10",null,"Oko lisovací z niklu do +650°C, průřez 95mm2 / M10 (65N10)","25ks",359.62011645902226,{"$f":"F1878*(1-Elteq!$F$9)","v":359.62011645902226},""]
["TECHNIK","OLN 95-M12",null,"Oko lisovací z niklu do +650°C, průřez 95mm2 / M12 (65N12)","25ks",361.84686640613694,{"$f":"F1879*(1-Elteq!$F$9)","v":361.84686640613694},"8591735056131"]
["TECHNIK","OLNO  2,5-M4",null,"Oko lisovací z nerezu do +450°C, průřez 1,5-2,5mm2 / svorník M4","100ks",204.48987014336558,{"$f":"F1880*(1-Elteq!$F$9)","v":204.48987014336558},"8591735029500"]
["TECHNIK","OLNO  2,5-M5",null,"Oko lisovací z nerezu do +450°C, průřez 1,5-2,5mm2 / svorník M5","100ks",204.48987014336558,{"$f":"F1881*(1-Elteq!$F$9)","v":204.48987014336558},"8591735029517"]
["TECHNIK","OLNO  2,5-M6",null,"Oko lisovací z nerezu do +450°C, průřez 1,5-2,5mm2 / svorník M6","100ks",206.71662009048026,{"$f":"F1882*(1-Elteq!$F$9)","v":206.71662009048026},"8591735029524"]
["TECHNIK","OLNO  6-M4",null,"Oko lisovací z nerezu do +450°C, průřez 4-6mm2 / svorník M4","100ks",222.3038697202831,{"$f":"F1883*(1-Elteq!$F$9)","v":222.3038697202831},"8591735029531"]
["TECHNIK","OLNO  6-M5",null,"Oko lisovací z nerezu do +450°C, průřez 4-6mm2 / svorník M5","100ks",224.15949467621201,{"$f":"F1884*(1-Elteq!$F$9)","v":224.15949467621201},"8591735029548"]
["TECHNIK","OLNO  6-M6",null,"Oko lisovací z nerezu do +450°C, průřez 4-6mm2 / svorník M6","100ks",228.24186957925559,{"$f":"F1885*(1-Elteq!$F$9)","v":228.24186957925559},"8591735029555"]
["TECHNIK","OLNO 10-M6",null,"Oko lisovací z nerezu do +450°C, průřez 10mm2 / svorník M6","100ks",285.39511822186591,{"$f":"F1886*(1-Elteq!$F$9)","v":285.39511822186591},"8591735037017"]
["TECHNIK","OLNO 10-M8",null,"Oko lisovací z nerezu do +450°C, průřez 10mm2 / svorník M8","100ks",285.39511822186591,{"$f":"F1887*(1-Elteq!$F$9)","v":285.39511822186591},"8591735029562"]
["TECHNIK","OLNO 16-M5",null,"Oko lisovací z nerezu do +450°C, průřez 16mm2 / svorník M5","100ks",295.04436799269627,{"$f":"F1888*(1-Elteq!$F$9)","v":295.04436799269627},"8591735029579"]
["TECHNIK","OLNO 16-M6",null,"Oko lisovací z nerezu do +450°C, průřez 16mm2 / svorník M6","100ks",303.20911779878344,{"$f":"F1889*(1-Elteq!$F$9)","v":303.20911779878344},"8591735029586"]
["TECHNIK","OLNO 16-M8",null,"Oko lisovací z nerezu do +450°C, průřez 16mm2 / svorník M8","100ks",327.33224222585926,{"$f":"F1890*(1-Elteq!$F$9)","v":327.33224222585926},"8591735029593"]
["TECHNIK","OLNO 50-M8",null,"Oko lisovací z nerezu do +450°C, průřez 50mm2 / svorník M8","50ks",480.97798857677276,{"$f":"F1891*(1-Elteq!$F$9)","v":480.97798857677276},"8591735056667"]
["TECHNIK","VNN  1,5-M4",null,"Vidlice lisovací z niklu do +650°C, průřez 0,5-1,5mm2 / M4","100ks",109.66743489539842,{"$f":"F1892*(1-Elteq!$F$9)","v":109.66743489539842},"8591735056056"]
["TECHNIK","VNN  1,5-M5",null,"Vidlice lisovací z niklu do +650°C, průřez 0,5-1,5mm2 / M5","100ks",112.079747338106,{"$f":"F1893*(1-Elteq!$F$9)","v":112.079747338106},"8591735056810"]
["TECHNIK","VNN  2,5-M4",null,"Vidlice lisovací z niklu do +650°C, průřez 1,5-2,5mm2 / M4","100ks",113.56424730284913,{"$f":"F1894*(1-Elteq!$F$9)","v":113.56424730284913},"8591735056834"]
["TECHNIK","VNN  2,5-M5",null,"Vidlice lisovací z niklu do +650°C, průřez 1,5-2,5mm2 / M5","100ks",115.23430976318514,{"$f":"F1895*(1-Elteq!$F$9)","v":115.23430976318514},"8591735056803"]
["TECHNIK","VNN  6-M5",null,"Vidlice lisovací z niklu do +650°C, průřez 4,0-6,0mm2 / M5","100ks",158.84149622751445,{"$f":"F1896*(1-Elteq!$F$9)","v":158.84149622751445},"8591735056827"]
["TECHNIK","AL 10",null,"Spojka lisovací Al do 1kV, průřez 10mm2","100ks",77.936248149014105,{"$f":"F1897*(1-Elteq!$F$9)","v":77.936248149014105},"8591735054281"]
["TECHNIK","AL 16",null,"Spojka lisovací Al do 1kV, průřez 16mm2","50ks",23.751999435890014,{"$f":"F1898*(1-Elteq!$F$9)","v":23.751999435890014},"8591735012946"]
["TECHNIK","AL 25",null,"Spojka lisovací Al do 1kV, průřez 25mm2","50ks",23.751999435890014,{"$f":"F1899*(1-Elteq!$F$9)","v":23.751999435890014},"8591735012939"]
["TECHNIK","AL 35",null,"Spojka lisovací Al do 1kV, průřez 35mm2","50ks",27.092124356562046,{"$f":"F1900*(1-Elteq!$F$9)","v":27.092124356562046},"8591735012922"]
["TECHNIK","AL 50",null,"Spojka lisovací Al do 1kV, průřez 50mm2","20ks",13.731624673873913,{"$f":"F1901*(1-Elteq!$F$9)","v":13.731624673873913},"8591735012762"]
["TECHNIK","AL 70",null,"Spojka lisovací Al do 1kV, průřez 70mm2","20ks",20.411874515217981,{"$f":"F1902*(1-Elteq!$F$9)","v":20.411874515217981},"8591735012915"]
["TECHNIK","AL 95",null,"Spojka lisovací Al do 1kV, průřez 95mm2","10ks",13.731624673873913,{"$f":"F1903*(1-Elteq!$F$9)","v":13.731624673873913},"8591735013851"]
["TECHNIK","AL120",null,"Spojka lisovací Al do 1kV, průřez 120mm2","10ks",13.731624673873913,{"$f":"F1904*(1-Elteq!$F$9)","v":13.731624673873913},"8591735012908"]
["TECHNIK","AL150",null,"Spojka lisovací Al do 1kV, průřez 150mm2","10ks",18.370687063696181,{"$f":"F1905*(1-Elteq!$F$9)","v":18.370687063696181},"8591735013318"]
["TECHNIK","AL185",null,"Spojka lisovací Al do 1kV, průřez 185mm2","10ks",22.824186957925559,{"$f":"F1906*(1-Elteq!$F$9)","v":22.824186957925559},"8591735013868"]
["TECHNIK","AL240",null,"Spojka lisovací Al do 1kV, průřez 240mm2","10ks",29.504436799269627,{"$f":"F1907*(1-Elteq!$F$9)","v":29.504436799269627},"8591735012779"]
["TECHNIK","AL300",null,"Spojka lisovací Al do 1kV, průřez 300mm2","10ks",34.885749171463459,{"$f":"F1908*(1-Elteq!$F$9)","v":34.885749171463459},"8591735027971"]
["TECHNIK","AL500",null,"Spojka lisovací Al do 1kV, průřez 500mm2","10ks",108.73962241743396,{"$f":"F1909*(1-Elteq!$F$9)","v":108.73962241743396},"8591735027964"]
["TECHNIK","AL-ZE 10",null,"Spojka lisovací Al s vazelínou do 10kV, průřez 10mm2","50ks",124.32687204723679,{"$f":"F1910*(1-Elteq!$F$9)","v":124.32687204723679},"8591735012892"]
["TECHNIK","AL-ZE 16",null,"Spojka lisovací Al s vazelínou do 10kV, průřez 16mm2","50ks",34.329061684684788,{"$f":"F1911*(1-Elteq!$F$9)","v":34.329061684684788},"8591735012885"]
["TECHNIK","AL-ZE 25",null,"Spojka lisovací Al s vazelínou do 10kV, průřez 25mm2","50ks",35.25687416264924,{"$f":"F1912*(1-Elteq!$F$9)","v":35.25687416264924},"8591735012878"]
["TECHNIK","AL-ZE 35",null,"Spojka lisovací Al s vazelínou do 10kV, průřez 35mm2","50ks",42.679373986364865,{"$f":"F1913*(1-Elteq!$F$9)","v":42.679373986364865},"8591735013875"]
["TECHNIK","AL-ZE 50",null,"Spojka lisovací Al s vazelínou do 10kV, průřez 50mm2","20ks",18.556249559289071,{"$f":"F1914*(1-Elteq!$F$9)","v":18.556249559289071},"8591735012861"]
["TECHNIK","AL-ZE 70",null,"Spojka lisovací Al s vazelínou do 10kV, průřez 70mm2","20ks",27.092124356562046,{"$f":"F1915*(1-Elteq!$F$9)","v":27.092124356562046},"8591735013882"]
["TECHNIK","AL-ZE 95",null,"Spojka lisovací Al s vazelínou do 10kV, průřez 95mm2","10ks",20.782999506403762,{"$f":"F1916*(1-Elteq!$F$9)","v":20.782999506403762},"8591735013899"]
["TECHNIK","AL-ZE120",null,"Spojka lisovací Al s vazelínou do 10kV, průřez 50mm2","10ks",20.040749524032197,{"$f":"F1917*(1-Elteq!$F$9)","v":20.040749524032197},"8591735012854"]
["TECHNIK","AL-ZE150",null,"Spojka lisovací Al s vazelínou do 10kV, průřez 150mm2","10ks",27.83437433893361,{"$f":"F1918*(1-Elteq!$F$9)","v":27.83437433893361},"8591735013905"]
["TECHNIK","AL-ZE185",null,"Spojka lisovací Al s vazelínou do 10kV, průřez 185mm2","10ks",33.40124920672033,{"$f":"F1919*(1-Elteq!$F$9)","v":33.40124920672033},"8591735013912"]
["TECHNIK","AL-ZE240",null,"Spojka lisovací Al s vazelínou do 10kV, průřez 240mm2","10ks",46.019498907036898,{"$f":"F1920*(1-Elteq!$F$9)","v":46.019498907036898},"8591735013202"]
["TECHNIK","AL-ZE300",null,"Spojka lisovací Al s vazelínou do 10kV, průřez 300mm2","10ks",59.379998589725034,{"$f":"F1921*(1-Elteq!$F$9)","v":59.379998589725034},"8591735040338"]
["TECHNIK","AL-ZE500",null,"Spojka lisovací Al s vazelínou do 10kV, průřez 500mm2","10ks",142.88312160652586,{"$f":"F1922*(1-Elteq!$F$9)","v":142.88312160652586},"8591735025757"]
["TECHNIK","KUR  2516",null,"Redukční spojka Cu, průřez 25/16mm2 jako vložka do Cu spojky KUZEV 25","25ks",38.596999083321272,{"$f":"F1923*(1-Elteq!$F$9)","v":38.596999083321272},"8591735051792"]
["TECHNIK","KUR  3525",null,"Redukční spojka Cu, průřez 35/25mm2 jako vložka do Cu spojky KUZEV 35","25ks",30.803374268419862,{"$f":"F1924*(1-Elteq!$F$9)","v":30.803374268419862},""]
["TECHNIK","KUR 12095",null,"Redukční spojka Cu, průřez 120/95mm2 jako vložka do Cu spojky KUZEV 120","25ks",43.792748959922214,{"$f":"F1925*(1-Elteq!$F$9)","v":43.792748959922214},"8591735056285"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"KUR 240185",null,"Redukční spojka Cu, průřez 240/185mm2 jako vložka do Cu spojky KUZEV 240","5ks",47.503998871780027,{"$f":"F1926*(1-Elteq!$F$9)","v":47.503998871780027},"8591735025702"]
["TECHNIK","KUR 300240",null,"Redukční spojka Cu, průřez 300/240mm2 jako vložka do Cu spojky KUZEV 300","5ks",65.132435953104647,{"$f":"F1927*(1-Elteq!$F$9)","v":65.132435953104647},""]
["TECHNIK","KUZEV  16",null,"Spojka Cu dle DIN 46267 cínovaná do 10kV, průřez 16mm2","100ks",77.936248149014105,{"$f":"F1928*(1-Elteq!$F$9)","v":77.936248149014105},"8591735045685"]
["TECHNIK","KUZEV  25",null,"Spojka Cu dle DIN 46267 cínovaná do 10kV, průřez 25mm2","50ks",60.122248572096595,{"$f":"F1929*(1-Elteq!$F$9)","v":60.122248572096595},"8591735046613"]
["TECHNIK","KUZEV  50",null,"Spojka Cu dle DIN 46267 cínovaná do 10kV, průřez 50mm2","50ks",110.96637236454866,{"$f":"F1930*(1-Elteq!$F$9)","v":110.96637236454866},"8591735046606"]
["TECHNIK","KUZEV 120",null,"Spojka Cu dle DIN 46267 cínovaná do 10kV, průřez 120mm2","25ks",82.389748043243486,{"$f":"F1931*(1-Elteq!$F$9)","v":82.389748043243486},"8591735056469"]
["TECHNIK","KUZEV 150",null,"Spojka Cu dle DIN 46267 cínovaná do 10kV, průřez 150mm2","10ks",44.349436446700885,{"$f":"F1932*(1-Elteq!$F$9)","v":44.349436446700885},"8591735054267"]
["TECHNIK","KUZEV 300",null,"Spojka Cu dle DIN 46267 cínovaná do 10kV, průřez 300mm2","10ks",101.68824758490412,{"$f":"F1933*(1-Elteq!$F$9)","v":101.68824758490412},"8591735046620"]
["TECHNIK","KUZEV 500",null,"Spojka Cu dle DIN 46267 cínovaná do 10kV, průřez 500mm2","10ks",293.11451803853021,{"$f":"F1934*(1-Elteq!$F$9)","v":293.11451803853021},"8591735046637"]
["TECHNIK","SL  0,5",null,"Spojka lehčená Cu pocínovaná, průřez 0,1-0,5mm2 / délka 12mm","100ks",3.8968124074507053,{"$f":"F1935*(1-Elteq!$F$9)","v":3.8968124074507053},"8591735004569"]
["TECHNIK","SL  0,75",null,"Spojka lehčená Cu pocínovaná, průřez 0,5-0,75mm2 / délka 14mm","100ks",5.5668748677867219,{"$f":"F1936*(1-Elteq!$F$9)","v":5.5668748677867219},"8591735053048"]
["TECHNIK","SL  1,5",null,"Spojka lehčená Cu pocínovaná, průřez 0,25-1,5mm2 / délka 15mm","100ks",6.1235623545653937,{"$f":"F1937*(1-Elteq!$F$9)","v":6.1235623545653937},"8591735004576"]
["TECHNIK","SL  1,5/20",null,"Spojka lehčená Cu pocínovaná, průřez 0,25-1,5mm2 / délka 20mm","100ks",7.236937328122738,{"$f":"F1938*(1-Elteq!$F$9)","v":7.236937328122738},"8591735026622"]
["TECHNIK","SL  1,5/25",null,"Spojka lehčená Cu pocínovaná, průřez 0,25-1,5mm2 / délka 25mm","100ks",7.0513748325298478,{"$f":"F1939*(1-Elteq!$F$9)","v":7.0513748325298478},"8591735055417"]
["TECHNIK","SL  2,5",null,"Spojka lehčená Cu pocínovaná, průřez 1,5-2,5mm2 / délka 15mm","100ks",7.6080623193085195,{"$f":"F1940*(1-Elteq!$F$9)","v":7.6080623193085195},"8591735004583"]
["TECHNIK","SL  2,5/20",null,"Spojka lehčená Cu pocínovaná, průřez 1,5-2,5mm2 / délka 20mm","100ks",8.5358747972729727,{"$f":"F1941*(1-Elteq!$F$9)","v":8.5358747972729727},"8591735007485"]
["TECHNIK","SL  2,5/25",null,"Spojka lehčená Cu pocínovaná, průřez 1,5-2,5mm2 / délka 25mm","100ks",8.3503123016800824,{"$f":"F1942*(1-Elteq!$F$9)","v":8.3503123016800824},"8591735055424"]
["TECHNIK","SL  4-6",null,"Spojka lehčená Cu pocínovaná, průřez 4-6mm2 / délka 15mm","100ks",10.762624744387661,{"$f":"F1943*(1-Elteq!$F$9)","v":10.762624744387661},"8591735004590"]
["TECHNIK","SL  4-6/20",null,"Spojka lehčená Cu pocínovaná, průřez 4-6mm2 / délka 20mm","100ks",11.504874726759224,{"$f":"F1944*(1-Elteq!$F$9)","v":11.504874726759224},"8591735013929"]
["TECHNIK","SL  6",null,"Spojka lehčená Cu pocínovaná, průřez 6,0mm2 / délka 20mm","100ks",44.534998942293775,{"$f":"F1945*(1-Elteq!$F$9)","v":44.534998942293775},"8591735054199"]
["TECHNIK","SL  6/25",null,"Spojka lehčená Cu pocínovaná, průřez 6,0mm2 / délka 25mm","100ks",47.875123862965808,{"$f":"F1946*(1-Elteq!$F$9)","v":47.875123862965808},"8591735004606"]
["TECHNIK","SL 10",null,"Spojka lehčená Cu pocínovaná, průřez 10mm2 / délka 30mm","100ks",48.988498836523149,{"$f":"F1947*(1-Elteq!$F$9)","v":48.988498836523149},"8591735004613"]
["TECHNIK","SL 16",null,"Spojka lehčená Cu pocínovaná, průřez 16mm2 / délka 35mm","100ks",57.153248642610343,{"$f":"F1948*(1-Elteq!$F$9)","v":57.153248642610343},"8591735004620"]
["TECHNIK","SL 25",null,"Spojka lehčená Cu pocínovaná, průřez 25mm2 / délka 40mm","50ks",32.287874233162988,{"$f":"F1949*(1-Elteq!$F$9)","v":32.287874233162988},"8591735004637"]
["TECHNIK","SL 35",null,"Spojka lehčená Cu pocínovaná, průřez 35mm2 / délka 45mm","50ks",38.040311596542601,{"$f":"F1950*(1-Elteq!$F$9)","v":38.040311596542601},"8591735004644"]
["TECHNIK","SL 50",null,"Spojka lehčená Cu pocínovaná, průřez 50mm2 / délka 50mm","50ks",60.493373563282375,{"$f":"F1951*(1-Elteq!$F$9)","v":60.493373563282375},"8591735004651"]
["TECHNIK","SL 70",null,"Spojka lehčená Cu pocínovaná, průřez 70mm2 / délka 55mm","50ks",82.575310538836376,{"$f":"F1952*(1-Elteq!$F$9)","v":82.575310538836376},"8591735004668"]
["TECHNIK","SL 95",null,"Spojka lehčená Cu pocínovaná, průřez 95mm2 / délka 60mm","25ks",46.390623898222685,{"$f":"F1953*(1-Elteq!$F$9)","v":46.390623898222685},"8591735004675"]
["TECHNIK","SL120",null,"Spojka lehčená Cu pocínovaná, průřez 120mm2 / délka 65mm","25ks",57.338811138203233,{"$f":"F1954*(1-Elteq!$F$9)","v":57.338811138203233},"8591735004682"]
["TECHNIK","SL150",null,"Spojka lehčená Cu pocínovaná, průřez 150mm2 / délka 70mm","10ks",29.689999294862517,{"$f":"F1955*(1-Elteq!$F$9)","v":29.689999294862517},"8591735004699"]
["TECHNIK","SL185",null,"Spojka lehčená Cu pocínovaná, průřez 185mm2 / délka 80mm","10ks",37.112499118578143,{"$f":"F1956*(1-Elteq!$F$9)","v":37.112499118578143},"8591735004705"]
["TECHNIK","SL240",null,"Spojka lehčená Cu pocínovaná, průřez 240mm2 / délka 90mm","10ks",47.503998871780027,{"$f":"F1957*(1-Elteq!$F$9)","v":47.503998871780027},"8591735004712"]
["TECHNIK","SL300",null,"Spojka lehčená Cu pocínovaná, průřez 300mm2 / délka 100mm","10ks",72.740498272413163,{"$f":"F1958*(1-Elteq!$F$9)","v":72.740498272413163},"8591735012731"]
["TECHNIK","SL400",null,"Spojka lehčená Cu pocínovaná, průřez 400mm2 / délka 110mm","10ks",86.843247937472867,{"$f":"F1959*(1-Elteq!$F$9)","v":86.843247937472867},"8591735007478"]
["TECHNIK","SL500",null,"Spojka lehčená Cu pocínovaná, průřez 500mm2 / délka 140mm","10ks",130.63599689739507,{"$f":"F1960*(1-Elteq!$F$9)","v":130.63599689739507},"8591735007461"]
["TECHNIK","SLP  0,5",null,"Spojka Cu paralelní pro celkový průřez 0,1-0,5mm2, délka 4,9mm","100ks",2.783437433893361,{"$f":"F1961*(1-Elteq!$F$9)","v":2.783437433893361},"8591735016319"]
["TECHNIK","SLP  0,5/5",null,"Spojka Cu paralelní pro celkový průřez 0,1-0,5mm2, délka 5mm (MOQ 2000ks)","100ks",2.9689999294862517,{"$f":"F1962*(1-Elteq!$F$9)","v":2.9689999294862517},"8591735048631"]
["TECHNIK","SLP  1,5",null,"Spojka Cu paralelní pro celkový průřez 0,25-1,5mm2, délka 8mm","100ks",3.5256874162649239,{"$f":"F1963*(1-Elteq!$F$9)","v":3.5256874162649239},"8591735011697"]
["TECHNIK","SLP  1,5/6",null,"Spojka Cu paralelní pro celkový průřez 0,25-1,5mm2, délka 6mm (MOQ 2000ks)","100ks",3.7112499118578146,{"$f":"F1964*(1-Elteq!$F$9)","v":3.7112499118578146},"8591735017064"]
["TECHNIK","SLP  2,5",null,"Spojka Cu paralelní pro celkový průřez 1,5-2,5mm2, délka 8mm","100ks",3.5256874162649239,{"$f":"F1965*(1-Elteq!$F$9)","v":3.5256874162649239},"8591735011703"]
["TECHNIK","SLP  2,5/6",null,"Spojka Cu paralelní pro celkový průřez 1,5-2,5mm2, délka 6mm (MOQ 2000ks)","100ks",3.7112499118578146,{"$f":"F1966*(1-Elteq!$F$9)","v":3.7112499118578146},"8591735017071"]
["TECHNIK","SLP  4-6",null,"Spojka Cu paralelní pro celkový průřez 4-6mm2, délka 9mm","100ks",5.0101873810080493,{"$f":"F1967*(1-Elteq!$F$9)","v":5.0101873810080493},"8591735011710"]
["TECHNIK","SLP  4-6/6",null,"Spojka Cu paralelní pro celkový průřez 4-6mm2, délka 6mm (MOQ 2000ks)","100ks",5.1957498766009405,{"$f":"F1968*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735017088"]
["TECHNIK","SLP 10",null,"Spojka Cu paralelní pro celkový průřez 10mm2, délka 10,5mm","100ks",11.504874726759224,{"$f":"F1969*(1-Elteq!$F$9)","v":11.504874726759224},"8591735007454"]
["TECHNIK","SLP 10/8",null,"Spojka Cu paralelní pro celkový průřez 10mm2, délka 8mm","100ks",17.9995620725104,{"$f":"F1970*(1-Elteq!$F$9)","v":17.9995620725104},"8591735025120"]
["TECHNIK","SLP 16",null,"Spojka Cu paralelní pro celkový průřez 16mm2, délka 11,5mm","100ks",16.700624603360165,{"$f":"F1971*(1-Elteq!$F$9)","v":16.700624603360165},"8591735010119"]
["TECHNIK","SLP 16/10",null,"Spojka Cu paralelní pro celkový průřez 16mm2, délka 10mm","100ks",20.226312019625091,{"$f":"F1972*(1-Elteq!$F$9)","v":20.226312019625091},"8591735029333"]
["TECHNIK","SLP 25",null,"Spojka Cu paralelní pro celkový průřez 25mm2, délka 13mm","100ks",30.803374268419862,{"$f":"F1973*(1-Elteq!$F$9)","v":30.803374268419862},"8591735014438"]
["TECHNIK","SLP 35",null,"Spojka Cu paralelní pro celkový průřez 35mm2, délka 14mm","100ks",41.565999012807524,{"$f":"F1974*(1-Elteq!$F$9)","v":41.565999012807524},"8591735027902"]
["TECHNIK","SLP 50",null,"Spojka Cu paralelní pro celkový průřez 50mm2, délka 16mm","100ks",71.627123298855821,{"$f":"F1975*(1-Elteq!$F$9)","v":71.627123298855821},"8591735017569"]
["TECHNIK","SLP 70",null,"Spojka Cu paralelní pro celkový průřez 70mm2, délka 25,7mm","50ks",55.29762368668144,{"$f":"F1976*(1-Elteq!$F$9)","v":55.29762368668144},"8591735051976"]
["TECHNIK","SLP 95",null,"Spojka Cu paralelní pro celkový průřez 95mm2, délka 21,7mm","50ks",60.864498554468156,{"$f":"F1977*(1-Elteq!$F$9)","v":60.864498554468156},"8591735054304"]
["TECHNIK","SLP120",null,"Spojka Cu paralelní pro celkový průřez 120mm2, délka 20mm","50ks",90.925622840516453,{"$f":"F1978*(1-Elteq!$F$9)","v":90.925622840516453},"8591735056445"]
["TECHNIK","SI  0,5/PA",null,"Lisovací spojka izolovaná, průřez 0,1-0,5mm2, izolace PA","100ks",5.3070873739566746,{"$f":"F1979*(1-Elteq!$F$9)","v":5.3070873739566746},"8591735004392"]
["TECHNIK","SI  1,5",null,"Lisovací spojka izolovaná, průřez 0,5-1,5mm2, izolace PVC","100ks",6.1235623545653937,{"$f":"F1980*(1-Elteq!$F$9)","v":6.1235623545653937},"8591735004408"]
["TECHNIK","SI  1,5/PA",null,"Lisovací spojka izolovaná, průřez 0,5-1,5mm2, izolace PA","100ks",9.5007997743560058,{"$f":"F1981*(1-Elteq!$F$9)","v":9.5007997743560058},"8591735015558"]
["TECHNIK","SI  1,5/PA/T",null,"Lisovací spojka izolovaná, průřez 0,5-1,5mm2, s nahlížecím otvorem, izolace PA","100ks",15.216124638617039,{"$f":"F1982*(1-Elteq!$F$9)","v":15.216124638617039},"8591735033743"]
["TECHNIK","SI  1,5/PC",null,"Lisovací spojka izolovaná, průřez 0,5-1,5mm2, izolace PC","100ks",9.649249770830318,{"$f":"F1983*(1-Elteq!$F$9)","v":9.649249770830318},"8591735004415"]
["TECHNIK","SI  2,5",null,"Lisovací spojka izolovaná, průřez 1,5-2,5mm2, izolace PVC","100ks",6.6802498413440663,{"$f":"F1984*(1-Elteq!$F$9)","v":6.6802498413440663},"8591735004422"]
["TECHNIK","SI  2,5/1,5",null,"Lisovací spojka izolovaná, redukce z 1,5-2,5mm2 na 0,5-1,5mm2, izolace PVC","100ks",20.894337003759496,{"$f":"F1985*(1-Elteq!$F$9)","v":20.894337003759496},"8591735034061"]
["TECHNIK","SI  2,5/PA",null,"Lisovací spojka izolovaná, průřez 1,5-2,5mm2, izolace PA","100ks",10.465724751439037,{"$f":"F1986*(1-Elteq!$F$9)","v":10.465724751439037},"8591735015923"]
["TECHNIK","SI  2,5/PA/T",null,"Lisovací spojka izolovaná, průřez 1,5-2,5mm2, s nahlížecím otvorem, izolace PA","100ks",17.81399957691751,{"$f":"F1987*(1-Elteq!$F$9)","v":17.81399957691751},"8591735033750"]
["TECHNIK","SI  2,5/PC",null,"Lisovací spojka izolovaná, průřez 1,5-2,5mm2, izolace PC","100ks",10.577062248794771,{"$f":"F1988*(1-Elteq!$F$9)","v":10.577062248794771},"8591735004439"]
["TECHNIK","SI  6",null,"Lisovací spojka izolovaná, průřez 4,0-6,0mm2, izolace PVC","100ks",10.020374762016099,{"$f":"F1989*(1-Elteq!$F$9)","v":10.020374762016099},"8591735004446"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"SI  6/1,5",null,"Lisovací spojka izolovaná, redukce z 4,0-6,0mm2 na 0,5-1,5mm2, izolace PVC","100ks",34.106386689973313,{"$f":"F1990*(1-Elteq!$F$9)","v":34.106386689973313},"8591735034078"]
["TECHNIK","SI  6/2,5",null,"Lisovací spojka izolovaná, redukce z 4,0-6,0mm2 na 1,5-2,5mm2, izolace PVC","100ks",27.314799351273514,{"$f":"F1991*(1-Elteq!$F$9)","v":27.314799351273514},"8591735034085"]
["TECHNIK","SI  6/32",null,"Lisovací spojka izolovaná, průřez 4,0-6,0mm2 / délka 32mm, izolace PVC","100ks",11.950224716182163,{"$f":"F1992*(1-Elteq!$F$9)","v":11.950224716182163},"8591735013998"]
["TECHNIK","SI  6/PA",null,"Lisovací spojka izolovaná, průřez 4,0-6,0mm2, izolace PA","100ks",15.401687134209931,{"$f":"F1993*(1-Elteq!$F$9)","v":15.401687134209931},"8591735015930"]
["TECHNIK","SI  6/PA/T",null,"Lisovací spojka izolovaná, průřez 4,0-6,0mm2 s nahlížecím otvorem, izolace PA","100ks",25.60762439181892,{"$f":"F1994*(1-Elteq!$F$9)","v":25.60762439181892},"8591735033767"]
["TECHNIK","SI  6/PC",null,"Lisovací spojka izolovaná, průřez 4,0-6,0mm2, izolace PC","100ks",14.39964965800832,{"$f":"F1995*(1-Elteq!$F$9)","v":14.39964965800832},"8591735004453"]
["TECHNIK","SI 10",null,"Lisovací spojka izolovaná, průřez 10mm2, izolace PVC červená","100ks",38.968124074507053,{"$f":"F1996*(1-Elteq!$F$9)","v":38.968124074507053},"8591735041168"]
["TECHNIK","SI 10/6",null,"Lisovací spojka izolovaná, redukce z 10mm2 na 6mm2, izolace PVC","10ks",6.2348998519211287,{"$f":"F1997*(1-Elteq!$F$9)","v":6.2348998519211287},"8591735051433"]
["TECHNIK","SI 10/PA",null,"Lisovací spojka izolovaná, průřez 10mm2, izolace PA","100ks",33.58681170231322,{"$f":"F1998*(1-Elteq!$F$9)","v":33.58681170231322},"8591735029241"]
["TECHNIK","SI 16",null,"Lisovací spojka izolovaná, průřez 16mm2, izolace PVC modrá","10ks",4.3792748959922214,{"$f":"F1999*(1-Elteq!$F$9)","v":4.3792748959922214},"8591735041175"]
["TECHNIK","SI 16/10",null,"Lisovací spojka izolovaná, redukce z 16mm2 na 10mm2, izolace PVC","10ks",7.274049827241317,{"$f":"F2000*(1-Elteq!$F$9)","v":7.274049827241317},"8591735051440"]
["TECHNIK","SI 16/PA",null,"Lisovací spojka izolovaná, průřez 16mm2, izolace PA","100ks",38.225874092135491,{"$f":"F2001*(1-Elteq!$F$9)","v":38.225874092135491},"8591735029258"]
["TECHNIK","SI 25",null,"Lisovací spojka izolovaná, průřez 25mm2, izolace PVC žlutá","10ks",14.585212153601212,{"$f":"F2002*(1-Elteq!$F$9)","v":14.585212153601212},"8591735041182"]
["TECHNIK","SI 25/PA",null,"Lisovací spojka izolovaná, průřez 25mm2, izolace PA žlutá (NL25)","25ks",33.957936693499001,{"$f":"F2003*(1-Elteq!$F$9)","v":33.957936693499001},"8591735056063"]
["TECHNIK","SI 35",null,"Lisovací spojka izolovaná, průřez 35mm2, izolace PVC červená","10ks",17.44287458573173,{"$f":"F2004*(1-Elteq!$F$9)","v":17.44287458573173},"8591735041199"]
["TECHNIK","SIK 1,5",null,"Lisovací spojka izolovaná, průřez 0,5-1,5mm2 pro mechanické zatížení, izolace PVC","100ks",7.3482748254784731,{"$f":"F2005*(1-Elteq!$F$9)","v":7.3482748254784731},"8591735017293"]
["TECHNIK","SIK 2,5",null,"Lisovací spojka izolovaná, průřez 1,5-2,5mm2 pro mechanické zatížení, izolace PVC","100ks",8.4987622981543947,{"$f":"F2006*(1-Elteq!$F$9)","v":8.4987622981543947},"8591735017378"]
["TECHNIK","SIK 6",null,"Lisovací spojka izolovaná, průřez 4,0-6,0mm2 pro mechanické zatížení, izolace PVC","100ks",16.700624603360165,{"$f":"F2007*(1-Elteq!$F$9)","v":16.700624603360165},"8591735017385"]
["TECHNIK","SIP 0,5/PA",null,"Lisovací spojka izolovaná paralelní, celkový průřez 0,1-0,5mm2, izolace PA","100ks",12.61824970031657,{"$f":"F2008*(1-Elteq!$F$9)","v":12.61824970031657},"8591735029203"]
["TECHNIK","SIP 1,5",null,"Lisovací spojka izolovaná paralelní, celkový průřez 0,5-1,5mm2, izolace PVC","100ks",4.5277248924665336,{"$f":"F2009*(1-Elteq!$F$9)","v":4.5277248924665336},"8591735004460"]
["TECHNIK","SIP 1,5/PA",null,"Lisovací spojka izolovaná paralelní, celkový průřez 0,5-1,5mm2, izolace PA","100ks",9.1667872822888015,{"$f":"F2010*(1-Elteq!$F$9)","v":9.1667872822888015},"8591735029210"]
["TECHNIK","SIP 2,5",null,"Lisovací spojka izolovaná paralelní, celkový průřez 1,5-2,5mm2, izolace PVC","100ks",5.3813123721938307,{"$f":"F2011*(1-Elteq!$F$9)","v":5.3813123721938307},"8591735004477"]
["TECHNIK","SIP 2,5/PA",null,"Lisovací spojka izolovaná paralelní, celkový průřez 1,5-2,5mm2, izolace PA","100ks",9.9461497637789424,{"$f":"F2012*(1-Elteq!$F$9)","v":9.9461497637789424},"8591735029227"]
["TECHNIK","SIP 6",null,"Lisovací spojka izolovaná paralelní, celkový průřez 4,0-6,0mm2, izolace PVC","100ks",7.0513748325298478,{"$f":"F2013*(1-Elteq!$F$9)","v":7.0513748325298478},"8591735004484"]
["TECHNIK","SIP 6/PA",null,"Lisovací spojka izolovaná paralelní, celkový průřez 4,0-6,0mm2, izolace PA","100ks",11.319312231166334,{"$f":"F2014*(1-Elteq!$F$9)","v":11.319312231166334},"8591735029234"]
["TECHNIK","SU  1,5",null,"Spojka ukončovací, průřez 0,5-1,5mm2, izolace PA","100ks",5.3070873739566746,{"$f":"F2015*(1-Elteq!$F$9)","v":5.3070873739566746},"8591735004521"]
["TECHNIK","SU  2,5",null,"Spojka ukončovací, průřez 1,0-2,5mm2, izolace PA","100ks",6.3462373492768629,{"$f":"F2016*(1-Elteq!$F$9)","v":6.3462373492768629},"8591735004538"]
["TECHNIK","SU  6",null,"Spojka ukončovací, průřez 2,5-6,0mm2, izolace PA","100ks",8.869887289340177,{"$f":"F2017*(1-Elteq!$F$9)","v":8.869887289340177},"8591735004545"]
["TECHNIK","SU 10",null,"Spojka ukončovací, průřez 4,0-10mm2, izolace PA","100ks",15.587249629802821,{"$f":"F2018*(1-Elteq!$F$9)","v":15.587249629802821},"8591735004552"]
["TECHNIK","LS  0,5",null,"Letovací spojka CWT se smršťovací bužírkou s lepidlem a tavnou pájkou, průřez 0,3-0,8mm2 (25ks)","25ks",12.061562213537897,{"$f":"F2019*(1-Elteq!$F$9)","v":12.061562213537897},"8591735026943"]
["TECHNIK","LS  0,5 / 100",null,"Letovací spojka CWT se smršťovací bužírkou s lepidlem a tavnou pájkou, průřez 0,3-0,8mm2","100ks",41.937124003993304,{"$f":"F2020*(1-Elteq!$F$9)","v":41.937124003993304},"8591735033262"]
["TECHNIK","LS  1,5",null,"Letovací spojka CWT se smršťovací bužírkou s lepidlem a tavnou pájkou, průřez 0,8-2,0mm2 (25ks)","25ks",12.98937469150235,{"$f":"F2021*(1-Elteq!$F$9)","v":12.98937469150235},"8591735018290"]
["TECHNIK","LS  1,5 / 100",null,"Letovací spojka CWT se smršťovací bužírkou s lepidlem a tavnou pájkou, průřez 0,8-2,0mm2","100ks",45.277248924665336,{"$f":"F2022*(1-Elteq!$F$9)","v":45.277248924665336},"8591735031428"]
["TECHNIK","LS  2,5",null,"Letovací spojka CWT se smršťovací bužírkou s lepidlem a tavnou pájkou, průřez 2,0-4,0mm2 (25ks)","25ks",13.917187169466805,{"$f":"F2023*(1-Elteq!$F$9)","v":13.917187169466805},"8591735018306"]
["TECHNIK","LS  2,5 / 100",null,"Letovací spojka CWT se smršťovací bužírkou s lepidlem a tavnou pájkou, průřez 2,0-4,0mm2","100ks",48.246248854151588,{"$f":"F2024*(1-Elteq!$F$9)","v":48.246248854151588},"8591735031435"]
["TECHNIK","LS  6",null,"Letovací spojka CWT se smršťovací bužírkou s lepidlem a tavnou pájkou, průřez 4,0-6,0mm2 (25ks)","25ks",15.772812125395712,{"$f":"F2025*(1-Elteq!$F$9)","v":15.772812125395712},"8591735018313"]
["TECHNIK","LS  6 / 100",null,"Letovací spojka CWT se smršťovací bužírkou s lepidlem a tavnou pájkou, průřez 4,0-6,0mm2","100ks",54.555373704309872,{"$f":"F2026*(1-Elteq!$F$9)","v":54.555373704309872},"8591735033279"]
["TECHNIK","LS 10",null,"Letovací spojka CWT se smršťovací bužírkou s lepidlem a tavnou pájkou, průřez 6,0-10mm2 (25ks)","25ks",16.143937116581494,{"$f":"F2027*(1-Elteq!$F$9)","v":16.143937116581494},"8591735028329"]
["TECHNIK","LS CWT-3809",null,"Letovací spojka CWT se smršťovací bužírkou a tavnou pájkou pro ukončení stínění kabelů 6,4-8,7mm","50ks",30.432249277234078,{"$f":"F2028*(1-Elteq!$F$9)","v":30.432249277234078},""]
["TECHNIK","LSD  0,5",null,"Letovací spojka se smršťovací bužírkou, průřez 2x0,15-2x0,4mm2, celkem 0,2-0,75mm2","50ks",36.370249136206581,{"$f":"F2029*(1-Elteq!$F$9)","v":36.370249136206581},"8591735045883"]
["TECHNIK","LSD  1,5",null,"Letovací spojka se smršťovací bužírkou, průřez 2x0,4-2x1,0mm2, celkem 0,6-2,0mm2 s dvojitou pájkou","50ks",29.875561790455407,{"$f":"F2030*(1-Elteq!$F$9)","v":29.875561790455407},"8591735028299"]
["TECHNIK","LSD  2,5",null,"Letovací spojka se smršťovací bužírkou, průřez 2x1,0-2x2,5mm2, celkem 1,8-2,5mm2 s dvojitou pájkou","50ks",33.215686711127439,{"$f":"F2031*(1-Elteq!$F$9)","v":33.215686711127439},"8591735028305"]
["TECHNIK","LSD  6",null,"Letovací spojka se smršťovací bužírkou, průřez 2x3,0-2x5,0mm2, celkem 2,4-4,5mm2 s dvojitou pájkou","50ks",37.669186605356821,{"$f":"F2032*(1-Elteq!$F$9)","v":37.669186605356821},"8591735028312"]
["TECHNIK","LSD-SET",null,"Sada letovacích spojek LSD pro průřezy 0,5-6mm2 (4 x 50ks)","1sada",125.9969345075728,{"$f":"F2033*(1-Elteq!$F$9)","v":125.9969345075728},"8591735031992"]
["TECHNIK","LS-SET",null,"Sada letovacích spojek LS pro průřezy 0,5-6mm2 (4 x 50ks)","1sada",72.740498272413163,{"$f":"F2034*(1-Elteq!$F$9)","v":72.740498272413163},"8591735032005"]
["TECHNIK","LS-SET-H",null,"Sada letovacích spojek LS pro průřezy 0,5-6mm2 (4 x 50ks) s hořákem","1sada",99.461497637789435,{"$f":"F2035*(1-Elteq!$F$9)","v":99.461497637789435},"8591735032012"]
["TECHNIK","SIS 0,5",null,"Spojka izolovaná smršťovací, průřez 0,1-0,5mm2, izolace PE","100ks",24.494249418261575,{"$f":"F2036*(1-Elteq!$F$9)","v":24.494249418261575},"8591735018320"]
["TECHNIK","SIS 1,5",null,"Spojka izolovaná smršťovací, průřez 0,5-1,5mm2, izolace PE","100ks",29.355986802795314,{"$f":"F2037*(1-Elteq!$F$9)","v":29.355986802795314},"8591735004491"]
["TECHNIK","SIS 2,5",null,"Spojka izolovaná smršťovací, průřez 1,5-2,5mm2, izolace PE","100ks",32.213649234925832,{"$f":"F2038*(1-Elteq!$F$9)","v":32.213649234925832},"8591735004507"]
["TECHNIK","SIS 2,5/1,5",null,"Spojka izolovaná smršťovací, redukce z 1,5-2,5mm2 na 0,5-1,5mm2, izolace PE","100ks",46.205061402629795,{"$f":"F2039*(1-Elteq!$F$9)","v":46.205061402629795},"8591735034092"]
["TECHNIK","SIS 6",null,"Spojka izolovaná smršťovací, průřez 4,0-6,0mm2, izolace PE","100ks",42.493811490771975,{"$f":"F2040*(1-Elteq!$F$9)","v":42.493811490771975},"8591735004514"]
["TECHNIK","SIS 6/2,5",null,"Spojka izolovaná smršťovací, redukce z 4,0-6,0mm2 na 1,5-2,5mm2, izolace PE","100ks",58.452186111760582,{"$f":"F2041*(1-Elteq!$F$9)","v":58.452186111760582},"8591735034108"]
["TECHNIK","SIS10",null,"Spojka izolovaná smršťovací, průřez 10mm2, izolace PE","10ks",7.979187310494301,{"$f":"F2042*(1-Elteq!$F$9)","v":7.979187310494301},"8591735033880"]
["TECHNIK","  156 SV-V",null,"Šroubová spojka s inbusovými šrouby na průřezy RE 1,5-6mm2, pro AL a CU vodiče do 1kV","1ks",2.1896374479961107,{"$f":"F2043*(1-Elteq!$F$9)","v":2.1896374479961107},"8591735040772"]
["TECHNIK","  250 SV-T-V-K",null,"Šroubová spojka s trhacími šrouby na průřezy SM 2,5-35mm2, RM 2,5-50mm2, pro AL a CU vodiče do 1kV","1ks",6.4946873457511751,{"$f":"F2044*(1-Elteq!$F$9)","v":6.4946873457511751},"8591735040550"]
["TECHNIK","  416 SV-V",null,"Šroubová spojka s inbusovými šrouby na průřezy RE/RM 1,5-16mm2, pro AL a CU vodiče do 1kV","1ks",2.3751999435890014,{"$f":"F2045*(1-Elteq!$F$9)","v":2.3751999435890014},"8591735029876"]
["TECHNIK","  625 SV-S-V",null,"Šroubová spojka s inbusovými šrouby na průřezy 4-35mm2, pro AL a CU vodiče do 1kV","1ks",2.9318874303676736,{"$f":"F2046*(1-Elteq!$F$9)","v":2.9318874303676736},"8591735038885"]
["TECHNIK","  625 SV-T-V-K",null,"Šroubová spojka s trhacími šrouby na průřezy 4-35mm2, pro AL a CU vodiče do 1kV","1ks",5.0472998801266282,{"$f":"F2047*(1-Elteq!$F$9)","v":5.0472998801266282},"8591735029883"]
["TECHNIK","  625 SV-V",null,"Šroubová spojka s inbusovými šrouby na průřezy RM 6-25mm2, RE 6-35mm2 pro AL a CU vodiče do 1kV","1ks",2.8576624321305171,{"$f":"F2048*(1-Elteq!$F$9)","v":2.8576624321305171},"8591735029906"]
["TECHNIK"," 1695 SV-T-V-K",null,"Šroubová spojka s trhacími šrouby na průřezy RM 16-95mm2, RE 16-50mm2 pro AL a CU vodiče do 1kV","1ks",5.8266623616167692,{"$f":"F2049*(1-Elteq!$F$9)","v":5.8266623616167692},"8591735029913"]
["TECHNIK"," 35185 SV-T-V-K",null,"Šroubová spojka s trhacími šrouby na průřezy RM 35-185mm2, RE 35-50mm2 pro AL a CU vodiče do 1kV","1ks",11.059524737336288,{"$f":"F2050*(1-Elteq!$F$9)","v":11.059524737336288},"8591735029920"]
["TECHNIK"," 50240 SV-T-V-K",null,"Šroubová spojka s trhacími šrouby na průřezy 50-240mm2, pro AL a CU vodiče do 1kV","1ks",32.955899217297393,{"$f":"F2051*(1-Elteq!$F$9)","v":32.955899217297393},"8591735049706"]
["TECHNIK","150240 SV-T-K",null,"Šroubová spojka s trhacími šrouby na průřezy RM/SM 150-240mm2, jen pro AL vodiče do 1kV","1ks",17.071749594545945,{"$f":"F2052*(1-Elteq!$F$9)","v":17.071749594545945},"8591735029937"]
["TECHNIK","150240 SV-T-V-K",null,"Šroubová spojka s trhacími šrouby na průřezy RM/SM 150-240mm2, pro AL a CU vodiče do 1kV","1ks",19.669624532846417,{"$f":"F2053*(1-Elteq!$F$9)","v":19.669624532846417},"8591735038441"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"M. 16-95",null,"Šroubová spojka s trhacími šrouby na průřezy 16-95mm2, pro AL a CU vodiče do 30kV, 2 šrouby","1ks",12.80381219590946,{"$f":"F2054*(1-Elteq!$F$9)","v":12.80381219590946},"8591735052652"]
["TECHNIK","M. 50-150",null,"Šroubová spojka s trhacími šrouby na průřezy 50-150mm2, pro AL a CU vodiče do 30kV, 2 šrouby","1ks",15.587249629802821,{"$f":"F2055*(1-Elteq!$F$9)","v":15.587249629802821},"8591735052669"]
["TECHNIK","M. 95-240",null,"Šroubová spojka s trhacími šrouby na průřezy 95-240mm2, pro AL a CU vodiče do 30kV, 4 šrouby","1ks",23.751999435890014,{"$f":"F2056*(1-Elteq!$F$9)","v":23.751999435890014},"8591735052676"]
["TECHNIK","M.120-300",null,"Šroubová spojka s trhacími šrouby na průřezy 120-300mm2, pro AL a CU vodiče do 30kV, 4 šrouby","1ks",30.246686781641188,{"$f":"F2057*(1-Elteq!$F$9)","v":30.246686781641188},"8591735052683"]
["TECHNIK","M.185-400",null,"Šroubová spojka s trhacími šrouby na průřezy 185-400mm2, pro AL a CU vodiče do 30kV, 6 šroubů","1ks",46.390623898222685,{"$f":"F2058*(1-Elteq!$F$9)","v":46.390623898222685},"8591735052690"]
["TECHNIK","SLN  1,5",null,"Spojky z niklu průřez 0,5-1,5mm2 do 650°C","100ks",110.96637236454866,{"$f":"F2059*(1-Elteq!$F$9)","v":110.96637236454866},"8591735032036"]
["TECHNIK","SLN  2,5",null,"Spojky z niklu průřez 1,5-2,5mm2 do 650°C","50ks",57.524373633796124,{"$f":"F2060*(1-Elteq!$F$9)","v":57.524373633796124},"8591735032043"]
["TECHNIK","SLN  6",null,"Spojky z niklu průřez 4,0-6,0mm2 do 650°C","50ks",60.307811067689485,{"$f":"F2061*(1-Elteq!$F$9)","v":60.307811067689485},"8591735032050"]
["TECHNIK","SLN 16",null,"Spojky z niklu průřez 16mm2 do 650°C","50ks",161.43937116581495,{"$f":"F2062*(1-Elteq!$F$9)","v":161.43937116581495},"8591735032067"]
["TECHNIK","451",null,"Spojka zkrucovací IDEAL s vnitřní pružinou, průřez 1,5-12mm2, barva žlutá","100ks",19.112937046067746,{"$f":"F2063*(1-Elteq!$F$9)","v":19.112937046067746},"8591735021009"]
["TECHNIK","452",null,"Spojka zkrucovací IDEAL s vnitřní pružinou, průřez 4,0-24mm2, barva rudá","100ks",27.64881184334072,{"$f":"F2064*(1-Elteq!$F$9)","v":27.64881184334072},"8591735021016"]
["TECHNIK","454",null,"Spojka zkrucovací IDEAL s vnitřní pružinou, průřez 12-36mm2, barva modrá","100ks",72.258035783871648,{"$f":"F2065*(1-Elteq!$F$9)","v":72.258035783871648},"8591735021023"]
["TECHNIK","71 B",null,"Spojka zkrucovací IDEAL s vnitřní pružinou, průřez 1,0-2,5mm2, barva šedá","100ks",10.243049756727569,{"$f":"F2066*(1-Elteq!$F$9)","v":10.243049756727569},"8591735021030"]
["TECHNIK","72 B",null,"Spojka zkrucovací IDEAL s vnitřní pružinou, průřez 1,5-3,5mm2, barva modrá","100ks",10.577062248794771,{"$f":"F2067*(1-Elteq!$F$9)","v":10.577062248794771},"8591735021047"]
["TECHNIK","73 B",null,"Spojka zkrucovací IDEAL s vnitřní pružinou, průřez 1,5-5,0mm2, barva oranžová","100ks",11.61621222411496,{"$f":"F2068*(1-Elteq!$F$9)","v":11.61621222411496},"8591735016579"]
["TECHNIK","74 B",null,"Spojka zkrucovací IDEAL s vnitřní pružinou, průřez 3,0-9,0mm2, barva žlutá","100ks",16.03259961922576,{"$f":"F2069*(1-Elteq!$F$9)","v":16.03259961922576},"8591735021054"]
["TECHNIK","76 B",null,"Spojka zkrucovací IDEAL s vnitřní pružinou, průřez 4,0-16mm2, barva rudá","100ks",22.267499471146888,{"$f":"F2070*(1-Elteq!$F$9)","v":22.267499471146888},"8591735016586"]
["TECHNIK","SZ  1,0-2,5",null,"Spojka zkrucovací s vnitřní pružinou, průřez 1,0-2,5mm2, barva šedá","100ks",4.5648373915851117,{"$f":"F2071*(1-Elteq!$F$9)","v":4.5648373915851117},"8591735009458"]
["TECHNIK","SZ  1,5-3,5",null,"Spojka zkrucovací s vnitřní pružinou, průřez 1,5-3,5mm2, barva modrá","100ks",4.9359623827708932,{"$f":"F2072*(1-Elteq!$F$9)","v":4.9359623827708932},"8591735020989"]
["TECHNIK","SZ  1,5-5",null,"Spojka zkrucovací s vnitřní pružinou, průřez 1,5-5,0mm2, barva oranžová, AKČNÍ CENA (MOQ 500ks)","100ks",2.1896374479961107,{"$f":"F2073*(1-Elteq!$F$9)","v":2.1896374479961107},"8591735009427"]
["TECHNIK","SZ  3-9",null,"Spojka zkrucovací s vnitřní pružinou, průřez 3,0-9,0mm2, barva žlutá","100ks",6.9771498342926916,{"$f":"F2074*(1-Elteq!$F$9)","v":6.9771498342926916},"8591735013493"]
["TECHNIK","SZ  4-16",null,"Spojka zkrucovací s vnitřní pružinou, průřez 4,0-16mm2, barva rudá","100ks",7.7193998166642546,{"$f":"F2075*(1-Elteq!$F$9)","v":7.7193998166642546},"8591735011000"]
["TECHNIK","SZ 10-21",null,"Spojka zkrucovací s vnitřní pružinou, průřez 10-21mm2, barva šedá","100ks",19.966524525795041,{"$f":"F2076*(1-Elteq!$F$9)","v":19.966524525795041},"8591735013509"]
["TECHNIK","SZT  1,5-10",null,"Spojka zkrucovací s vnitřní pružinou, průřez 1,5-10mm2, barva žlutá","100ks",7.6080623193085195,{"$f":"F2077*(1-Elteq!$F$9)","v":7.6080623193085195},"8591735013516"]
["TECHNIK","SZT  4-21",null,"Spojka zkrucovací s vnitřní pružinou, průřez 4,0-21mm2, barva rudá","100ks",9.1296747831702234,{"$f":"F2078*(1-Elteq!$F$9)","v":9.1296747831702234},"8591735013523"]
["TECHNIK","SZT 10-30",null,"Spojka zkrucovací s vnitřní pružinou, průřez 10-30mm2, barva modrá","100ks",24.38291192090584,{"$f":"F2079*(1-Elteq!$F$9)","v":24.38291192090584},"8591735013530"]
["TECHNIK","TWISTER 341",null,"Spojka zkrucovací IDEAL s vnitřní pružinou, průřez 1,0-15mm2, barva žluto-hnědá (MOQ 5000ks)","100ks",15.401687134209931,{"$f":"F2080*(1-Elteq!$F$9)","v":15.401687134209931},"8591735009434"]
["TECHNIK","TWISTER 342",null,"Spojka zkrucovací IDEAL s vnitřní pružinou, průřez 5,0-23mm2, barva šedá","100ks",42.01134900223046,{"$f":"F2081*(1-Elteq!$F$9)","v":42.01134900223046},"8591735009441"]
["TECHNIK","TWISTER 344 PRO",null,"Spojka zkrucovací IDEAL s vnitřní pružinou, průřez 1,5-24mm2, barva červeno-černá","100ks",34.069274190854735,{"$f":"F2082*(1-Elteq!$F$9)","v":34.069274190854735},"8591735020996"]
["TECHNIK","KES 2x2,5",null,"Krabicová bezšroubová elektrosvorka typu PC252, průřez 2x1,0-2,5mm2, barva rudá","100ks",7.4224998237156292,{"$f":"F2083*(1-Elteq!$F$9)","v":7.4224998237156292},"8591735020927"]
["TECHNIK","KES 3x2,5",null,"Krabicová bezšroubová elektrosvorka typu PC253, průřez 3x1,0-2,5mm2, barva oranžová","100ks",8.7214372928658648,{"$f":"F2084*(1-Elteq!$F$9)","v":8.7214372928658648},"8591735020934"]
["TECHNIK","KES 4x2,5",null,"Krabicová bezšroubová elektrosvorka typu PC254, průřez 4x1,0-2,5mm2, barva žlutá","100ks",11.504874726759224,{"$f":"F2085*(1-Elteq!$F$9)","v":11.504874726759224},"8591735020941"]
["TECHNIK","KES 5x2,5",null,"Krabicová bezšroubová elektrosvorka typu PC255, průřez 5x1,0-2,5mm2, barva šedá","100ks",12.247124709130787,{"$f":"F2086*(1-Elteq!$F$9)","v":12.247124709130787},"8591735020958"]
["TECHNIK","KES 6x2,5",null,"Krabicová bezšroubová elektrosvorka typu PC256, průřez 6x1,0-2,5mm2, barva modrá","100ks",21.154124497589542,{"$f":"F2087*(1-Elteq!$F$9)","v":21.154124497589542},"8591735020965"]
["TECHNIK","KES 8x2,5",null,"Krabicová bezšroubová elektrosvorka typu PC258, průřez 8x1,0-2,5mm2, barva černá","100ks",21.896374479961107,{"$f":"F2088*(1-Elteq!$F$9)","v":21.896374479961107},"8591735020972"]
["TECHNIK","KLE 2,5",null,"Zářezová svorka Cu pro průřezy 2,5mm2","100ks",38.596999083321272,{"$f":"F2089*(1-Elteq!$F$9)","v":38.596999083321272},"8591735032029"]
["TECHNIK","ZS 1",null,"Zářezová svorka odbočná, průřez 0,5-1,0mm2","100ks",6.3091248501582848,{"$f":"F2090*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735006877"]
["TECHNIK","ZS 2,5",null,"Zářezová svorka odbočná, průřez 1,5-2,5mm2","100ks",6.3091248501582848,{"$f":"F2091*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735006884"]
["TECHNIK","ZS 6",null,"Zářezová svorka odbočná, průřez 4,0-6,0mm2","100ks",11.504874726759224,{"$f":"F2092*(1-Elteq!$F$9)","v":11.504874726759224},"8591735006891"]
["TECHNIK","ZSD 1",null,"Zářezová svorka dvojitá odbočná, průřez 0,5-1,5mm2","100ks",13.360499682688133,{"$f":"F2093*(1-Elteq!$F$9)","v":13.360499682688133},"8591735016593"]
["TECHNIK","ZSD 2,5",null,"Zářezová svorka dvojitá odbočná, průřez 1,5-2,5mm2","100ks",15.587249629802821,{"$f":"F2094*(1-Elteq!$F$9)","v":15.587249629802821},"8591735016609"]
["TECHNIK","ZSD 4",null,"Zářezová svorka dvojitá odbočná, průřez 3,0-4,0mm2 / odbočný vodič 0,75-1,5mm2","100ks",31.916749241977204,{"$f":"F2095*(1-Elteq!$F$9)","v":31.916749241977204},"8591735041144"]
["TECHNIK","ZSP 2",null,"Zářezová svorka pro pojistku, průřez 0,8-2,0mm2","25ks",7.7936248149014107,{"$f":"F2096*(1-Elteq!$F$9)","v":7.7936248149014107},"8591735006907"]
["TECHNIK","VI  0,5-M 2/PA",null,"Vidlice izolovaná Cu, průřez 0,2-0,5mm2 / M2 / šíře 5mm, izolace PA","100ks",4.824624885415159,{"$f":"F2097*(1-Elteq!$F$9)","v":4.824624885415159},"8591735009816"]
["TECHNIK","VI  0,5-M 3,5/PA",null,"Vidlice izolovaná Cu, průřez 0,2-0,5mm2 / M3,5 / šíře 6mm, izolace PA","100ks",4.824624885415159,{"$f":"F2098*(1-Elteq!$F$9)","v":4.824624885415159},"8591735009878"]
["TECHNIK","VI  0,5-M 3/PA",null,"Vidlice izolovaná Cu, průřez 0,2-0,5mm2 / M3 / šíře 5mm, izolace PA","100ks",4.824624885415159,{"$f":"F2099*(1-Elteq!$F$9)","v":4.824624885415159},"8591735009861"]
["TECHNIK","VI  0,5-M 4/PA",null,"Vidlice izolovaná Cu, průřez 0,2-0,5mm2 / M4 / šíře 6,5mm, izolace PA","100ks",4.824624885415159,{"$f":"F2100*(1-Elteq!$F$9)","v":4.824624885415159},"8591735009885"]
["TECHNIK","VI  0,5-M 5/PA",null,"Vidlice izolovaná Cu, průřez 0,2-0,5mm2 / M5 / šíře 8mm, izolace PA","100ks",4.824624885415159,{"$f":"F2101*(1-Elteq!$F$9)","v":4.824624885415159},"8591735009892"]
["TECHNIK","VI  1,5-M 3",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M3 / šíře 6mm, izolace PVC","100ks",3.4885749171463458,{"$f":"F2102*(1-Elteq!$F$9)","v":3.4885749171463458},"8591735005634"]
["TECHNIK","VI  1,5-M 3,5",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M3,5 / šíře 6mm, izolace PVC","100ks",3.5256874162649239,{"$f":"F2103*(1-Elteq!$F$9)","v":3.5256874162649239},"8591735003807"]
["TECHNIK","VI  1,5-M 3,5/E",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M3,5 / šíře 6mm, izolace PVC","100ks",3.8225874092135492,{"$f":"F2104*(1-Elteq!$F$9)","v":3.8225874092135492},"8591735019648"]
["TECHNIK","VI  1,5-M 3,5/PA",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M3,5 / šíře 6mm, izolace PA","100ks",7.0884873316484258,{"$f":"F2105*(1-Elteq!$F$9)","v":7.0884873316484258},"8591735020156"]
["TECHNIK","VI  1,5-M 3,5/PC",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M3,5 / šíře 6mm, izolace PC","100ks",6.3091248501582848,{"$f":"F2106*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735010874"]
["TECHNIK","VI  1,5-M 3/E",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M3 / šíře 6mm, izolace PVC","100ks",3.8225874092135492,{"$f":"F2107*(1-Elteq!$F$9)","v":3.8225874092135492},"8591735019655"]
["TECHNIK","VI  1,5-M 3/PA",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M3 / šíře 6mm, izolace PA","100ks",6.383349848395441,{"$f":"F2108*(1-Elteq!$F$9)","v":6.383349848395441},"8591735020163"]
["TECHNIK","VI  1,5-M 3/PC",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M3 / šíře 6mm, izolace PC","100ks",6.3091248501582848,{"$f":"F2109*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735010867"]
["TECHNIK","VI  1,5-M 4",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M4 / šíře 6,8mm, izolace PVC","100ks",3.59991241450208,{"$f":"F2110*(1-Elteq!$F$9)","v":3.59991241450208},"8591735003814"]
["TECHNIK","VI  1,5-M 4/8",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M4 / šíře 8,1mm, izolace PVC","100ks",3.6741374127392366,{"$f":"F2111*(1-Elteq!$F$9)","v":3.6741374127392366},"8591735025427"]
["TECHNIK","VI  1,5-M 4/8/PA",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M4 / šíře 8,1mm, izolace PA","100ks",7.3853873245970512,{"$f":"F2112*(1-Elteq!$F$9)","v":7.3853873245970512},"8591735055608"]
["TECHNIK","VI  1,5-M 4/PA",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M4 / šíře 7mm, izolace PA","100ks",7.19982482900416,{"$f":"F2113*(1-Elteq!$F$9)","v":7.19982482900416},"8591735020170"]
["TECHNIK","VI  1,5-M 4/PC",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M4 / šíře 8mm, izolace PC","100ks",6.9400373351741136,{"$f":"F2114*(1-Elteq!$F$9)","v":6.9400373351741136},"8591735010881"]
["TECHNIK","VI  1,5-M 5",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M5 / šíře 8mm, izolace PVC","100ks",3.8968124074507053,{"$f":"F2115*(1-Elteq!$F$9)","v":3.8968124074507053},"8591735003821"]
["TECHNIK","VI  1,5-M 5/10",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M5 / šíře 9,5mm, izolace PVC","100ks",4.00814990480644,{"$f":"F2116*(1-Elteq!$F$9)","v":4.00814990480644},"8591735025410"]
["TECHNIK","VI  1,5-M 5/E",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M5 / šíře 10mm, izolace PVC","100ks",4.2679373986364864,{"$f":"F2117*(1-Elteq!$F$9)","v":4.2679373986364864},"8591735019662"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"VI  1,5-M 5/PA",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M5 / šíře 9,5mm, izolace PA","100ks",7.274049827241317,{"$f":"F2118*(1-Elteq!$F$9)","v":7.274049827241317},"8591735020187"]
["TECHNIK","VI  1,5-M 5/PC",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M5 / šíře 10mm, izolace PC","100ks",7.4967248219527853,{"$f":"F2119*(1-Elteq!$F$9)","v":7.4967248219527853},"8591735010898"]
["TECHNIK","VI  1,5-M 6",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M6 / šíře 12mm, izolace PVC","100ks",5.7524373633796122,{"$f":"F2120*(1-Elteq!$F$9)","v":5.7524373633796122},"8591735003838"]
["TECHNIK","VI  1,5-M 6/10",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M6 / šíře 9,5mm, izolace PVC","100ks",5.7524373633796122,{"$f":"F2121*(1-Elteq!$F$9)","v":5.7524373633796122},"8591735025434"]
["TECHNIK","VI  1,5-M 6/E",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M6 / šíře 11mm, izolace PVC","100ks",6.0122248572096595,{"$f":"F2122*(1-Elteq!$F$9)","v":6.0122248572096595},"8591735019679"]
["TECHNIK","VI  1,5-M 6/PA",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M6 / šíře 12mm, izolace PA","100ks",8.869887289340177,{"$f":"F2123*(1-Elteq!$F$9)","v":8.869887289340177},"8591735020194"]
["TECHNIK","VI  1,5-M 6/PC",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M6 / šíře 11mm, izolace PC","100ks",10.762624744387661,{"$f":"F2124*(1-Elteq!$F$9)","v":10.762624744387661},"8591735010904"]
["TECHNIK","VI  1,5-M 8",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M8 / šíře 14mm, izolace PVC","100ks",8.5358747972729727,{"$f":"F2125*(1-Elteq!$F$9)","v":8.5358747972729727},"8591735003845"]
["TECHNIK","VI  1,5-M10",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M10 / šíře 18mm, izolace PVC","100ks",20.894337003759496,{"$f":"F2126*(1-Elteq!$F$9)","v":20.894337003759496},"8591735003852"]
["TECHNIK","VI  1,5-M12",null,"Vidlice izolovaná Cu, průřez 0,5-1,5mm2 / M12 / šíře 20mm, izolace PVC","100ks",22.23038697202831,{"$f":"F2127*(1-Elteq!$F$9)","v":22.23038697202831},"8591735003869"]
["TECHNIK","VI  2,5-M 3",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M3 / šíře 6mm, izolace PVC","100ks",4.4534998942293775,{"$f":"F2128*(1-Elteq!$F$9)","v":4.4534998942293775},"8591735003876"]
["TECHNIK","VI  2,5-M 3,5",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M3,5 / šíře 6mm, izolace PVC","100ks",4.5277248924665336,{"$f":"F2129*(1-Elteq!$F$9)","v":4.5277248924665336},"8591735003883"]
["TECHNIK","VI  2,5-M 3,5/E",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M3,5 / šíře 6mm, izolace PVC","100ks",4.8988498836523151,{"$f":"F2130*(1-Elteq!$F$9)","v":4.8988498836523151},"8591735019686"]
["TECHNIK","VI  2,5-M 3,5/PA",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M3,5 / šíře 6,4mm, izolace PA","100ks",8.2018623052057702,{"$f":"F2131*(1-Elteq!$F$9)","v":8.2018623052057702},"8591735020200"]
["TECHNIK","VI  2,5-M 3,5/PC",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M3,5 / šíře 6mm, izolace PC","100ks",7.236937328122738,{"$f":"F2132*(1-Elteq!$F$9)","v":7.236937328122738},"8591735011789"]
["TECHNIK","VI  2,5-M 3/E",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M3 / šíře 5,8mm, izolace PVC","100ks",4.824624885415159,{"$f":"F2133*(1-Elteq!$F$9)","v":4.824624885415159},"8591735019693"]
["TECHNIK","VI  2,5-M 3/PA",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M3 / šíře 5,8mm, izolace PA","100ks",7.4224998237156292,{"$f":"F2134*(1-Elteq!$F$9)","v":7.4224998237156292},"8591735020217"]
["TECHNIK","VI  2,5-M 3/PC",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M3 / šíře 6mm, izolace PC","100ks",6.383349848395441,{"$f":"F2135*(1-Elteq!$F$9)","v":6.383349848395441},"8591735011772"]
["TECHNIK","VI  2,5-M 4",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M4 / šíře 7,2mm, izolace PVC","100ks",4.4534998942293775,{"$f":"F2136*(1-Elteq!$F$9)","v":4.4534998942293775},"8591735003890"]
["TECHNIK","VI  2,5-M 4/6",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M4 / šíře 6,8mm, izolace PVC","100ks",4.5277248924665336,{"$f":"F2137*(1-Elteq!$F$9)","v":4.5277248924665336},"8591735030025"]
["TECHNIK","VI  2,5-M 4/8",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M4 / šíře 8mm, izolace PVC","100ks",4.5277248924665336,{"$f":"F2138*(1-Elteq!$F$9)","v":4.5277248924665336},"8591735025441"]
["TECHNIK","VI  2,5-M 4/E",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M4 / šíře 8mm, izolace PVC","100ks",4.861737384533737,{"$f":"F2139*(1-Elteq!$F$9)","v":4.861737384533737},"8591735019709"]
["TECHNIK","VI  2,5-M 4/PA",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M4 / šíře 7,2mm, izolace PA","100ks",8.4245372999172385,{"$f":"F2140*(1-Elteq!$F$9)","v":8.4245372999172385},"8591735020224"]
["TECHNIK","VI  2,5-M 4/PC",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M4 / šíře 8mm, izolace PC","100ks",7.311162326359895,{"$f":"F2141*(1-Elteq!$F$9)","v":7.311162326359895},"8591735010911"]
["TECHNIK","VI  2,5-M 5",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M5 / šíře 8,5mm, izolace PVC","100ks",4.7132873880594248,{"$f":"F2142*(1-Elteq!$F$9)","v":4.7132873880594248},"8591735003906"]
["TECHNIK","VI  2,5-M 5/10",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M5 / šíře 10mm, izolace PVC","100ks",4.824624885415159,{"$f":"F2143*(1-Elteq!$F$9)","v":4.824624885415159},"8591735019600"]
["TECHNIK","VI  2,5-M 5/10/E",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M5 / šíře 10mm, izolace PVC","100ks",5.1215248783637843,{"$f":"F2144*(1-Elteq!$F$9)","v":5.1215248783637843},"8591735019716"]
["TECHNIK","VI  2,5-M 5/10/PA",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M5 / šíře 9,5mm, izolace PA","100ks",9.0554497849330673,{"$f":"F2145*(1-Elteq!$F$9)","v":9.0554497849330673},"8591735020231"]
["TECHNIK","VI  2,5-M 5/10/PC",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M5 / šíře 10mm, izolace PC","100ks",8.1276373069686141,{"$f":"F2146*(1-Elteq!$F$9)","v":8.1276373069686141},"8591735010928"]
["TECHNIK","VI  2,5-M 5/10/PK",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M5 / šíře 10mm, izolace PC","100ks",9.1667872822888015,{"$f":"F2147*(1-Elteq!$F$9)","v":9.1667872822888015},"8591735040185"]
["TECHNIK","VI  2,5-M 6",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M6 / šíře 12mm, izolace PVC","100ks",5.3441998730752527,{"$f":"F2148*(1-Elteq!$F$9)","v":5.3441998730752527},"8591735003920"]
["TECHNIK","VI  2,5-M 6/10",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M6 / šíře 9,5mm, izolace PVC","100ks",5.4555373704309877,{"$f":"F2149*(1-Elteq!$F$9)","v":5.4555373704309877},"8591735025458"]
["TECHNIK","VI  2,5-M 6/E",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M6 / šíře 11mm, izolace PVC","100ks",5.7524373633796122,{"$f":"F2150*(1-Elteq!$F$9)","v":5.7524373633796122},"8591735019723"]
["TECHNIK","VI  2,5-M 6/PA",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M6 / šíře 11mm, izolace PA","100ks",9.5379122734745838,{"$f":"F2151*(1-Elteq!$F$9)","v":9.5379122734745838},"8591735020248"]
["TECHNIK","VI  2,5-M 6/PC",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M6 / šíře 11mm, izolace PC","100ks",8.5729872963915525,{"$f":"F2152*(1-Elteq!$F$9)","v":8.5729872963915525},"8591735010935"]
["TECHNIK","VI  2,5-M 8",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M8 / šíře 14mm, izolace PVC","100ks",9.0183372858144892,{"$f":"F2153*(1-Elteq!$F$9)","v":9.0183372858144892},"8591735003944"]
["TECHNIK","VI  2,5-M10",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M10 / šíře 18mm, izolace PVC","100ks",18.890262051356277,{"$f":"F2154*(1-Elteq!$F$9)","v":18.890262051356277},"8591735003951"]
["TECHNIK","VI  2,5-M12",null,"Vidlice izolovaná Cu, průřez 1,5-2,5mm2 / M12 / šíře 20mm, izolace PVC","100ks",26.980786859206312,{"$f":"F2155*(1-Elteq!$F$9)","v":26.980786859206312},"8591735003968"]
["TECHNIK","VI  6-M 3",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M3 / šíře 6mm, izolace PVC","100ks",7.274049827241317,{"$f":"F2156*(1-Elteq!$F$9)","v":7.274049827241317},"8591735017309"]
["TECHNIK","VI  6-M 3,5",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M3,5 / šíře 6mm, izolace PVC","100ks",7.0513748325298478,{"$f":"F2157*(1-Elteq!$F$9)","v":7.0513748325298478},"8591735003975"]
["TECHNIK","VI  6-M 3,5/E",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M3,5 / šíře 6,4mm, izolace PVC","100ks",7.5709498201899414,{"$f":"F2158*(1-Elteq!$F$9)","v":7.5709498201899414},"8591735019730"]
["TECHNIK","VI  6-M 3,5/PA",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M3,5 / šíře 8,3mm, izolace PA","100ks",8.4616497990358166,{"$f":"F2159*(1-Elteq!$F$9)","v":8.4616497990358166},"8591735020255"]
["TECHNIK","VI  6-M 3,5/PC",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M3,5 / šíře 6,4mm, izolace PC","100ks",9.2410122805259576,{"$f":"F2160*(1-Elteq!$F$9)","v":9.2410122805259576},"8591735011796"]
["TECHNIK","VI  6-M 3/E",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M3 / šíře 6mm, izolace PVC","100ks",7.5709498201899414,{"$f":"F2161*(1-Elteq!$F$9)","v":7.5709498201899414},"8591735019747"]
["TECHNIK","VI  6-M 4",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M4 / šíře 8mm, izolace PVC","100ks",7.0513748325298478,{"$f":"F2162*(1-Elteq!$F$9)","v":7.0513748325298478},"8591735003982"]
["TECHNIK","VI  6-M 4/10",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M4 / šíře 9,5mm, izolace PVC","100ks",7.5709498201899414,{"$f":"F2163*(1-Elteq!$F$9)","v":7.5709498201899414},"8591735025465"]
["TECHNIK","VI  6-M 4/7",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M4 / šíře 7mm, izolace PVC","100ks",7.0513748325298478,{"$f":"F2164*(1-Elteq!$F$9)","v":7.0513748325298478},"8591735025472"]
["TECHNIK","VI  6-M 4/7/E",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M4 / šíře 7mm, izolace PVC","100ks",7.5709498201899414,{"$f":"F2165*(1-Elteq!$F$9)","v":7.5709498201899414},"8591735028459"]
["TECHNIK","VI  6-M 4/8/PC",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M4 / šíře 8mm, izolace PC","100ks",9.2410122805259576,{"$f":"F2166*(1-Elteq!$F$9)","v":9.2410122805259576},"8591735010942"]
["TECHNIK","VI  6-M 4/E",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M4 / šíře 10mm, izolace PVC","100ks",7.5709498201899414,{"$f":"F2167*(1-Elteq!$F$9)","v":7.5709498201899414},"8591735019754"]
["TECHNIK","VI  6-M 4/PA",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M4 / šíře 10mm, izolace PA","100ks",9.5007997743560058,{"$f":"F2168*(1-Elteq!$F$9)","v":9.5007997743560058},"8591735020262"]
["TECHNIK","VI  6-M 5",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M5 / šíře 10mm, izolace PVC","100ks",7.0513748325298478,{"$f":"F2169*(1-Elteq!$F$9)","v":7.0513748325298478},"8591735003999"]
["TECHNIK","VI  6-M 5/E",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M5 / šíře 10mm, izolace PVC","100ks",7.5709498201899414,{"$f":"F2170*(1-Elteq!$F$9)","v":7.5709498201899414},"8591735019761"]
["TECHNIK","VI  6-M 5/PA",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M5 / šíře 10mm, izolace PA","100ks",9.9832622628975205,{"$f":"F2171*(1-Elteq!$F$9)","v":9.9832622628975205},"8591735020279"]
["TECHNIK","VI  6-M 5/PC",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M5 / šíře 10mm, izolace PC","100ks",9.2410122805259576,{"$f":"F2172*(1-Elteq!$F$9)","v":9.2410122805259576},"8591735010959"]
["TECHNIK","VI  6-M 6",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M6 / šíře 11mm, izolace PVC","100ks",8.5358747972729727,{"$f":"F2173*(1-Elteq!$F$9)","v":8.5358747972729727},"8591735004002"]
["TECHNIK","VI  6-M 6/E",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M6 / šíře 11mm, izolace PVC","100ks",8.9441122875773331,{"$f":"F2174*(1-Elteq!$F$9)","v":8.9441122875773331},"8591735019778"]
["TECHNIK","VI  6-M 6/PA",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M6 / šíře 11mm, izolace PA","100ks",10.762624744387661,{"$f":"F2175*(1-Elteq!$F$9)","v":10.762624744387661},"8591735020286"]
["TECHNIK","VI  6-M 6/PC",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M6 / šíře 11mm, izolace PC","100ks",10.948187239980554,{"$f":"F2176*(1-Elteq!$F$9)","v":10.948187239980554},"8591735010966"]
["TECHNIK","VI  6-M 8",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M8 / šíře 14mm, izolace PVC","100ks",13.249162185332398,{"$f":"F2177*(1-Elteq!$F$9)","v":13.249162185332398},"8591735004019"]
["TECHNIK","VI  6-M 8/E",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M8 / šíře 14mm, izolace PVC","100ks",13.583174677399601,{"$f":"F2178*(1-Elteq!$F$9)","v":13.583174677399601},"8591735019785"]
["TECHNIK","VI  6-M 8/PA",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M8 / šíře 14mm, izolace PA","100ks",16.069712118344338,{"$f":"F2179*(1-Elteq!$F$9)","v":16.069712118344338},"8591735020293"]
["TECHNIK","VI  6-M 8/PC",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M8 / šíře 14mm, izolace PC","100ks",14.436762157126898,{"$f":"F2180*(1-Elteq!$F$9)","v":14.436762157126898},"8591735010973"]
["TECHNIK","VI  6-M10",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M10 / šíře 18mm, izolace PVC","100ks",15.884149622751446,{"$f":"F2181*(1-Elteq!$F$9)","v":15.884149622751446},"8591735004026"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"VI  6-M10/PA",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M10 / šíře 18mm, izolace PA","100ks",18.370687063696181,{"$f":"F2182*(1-Elteq!$F$9)","v":18.370687063696181},"8591735055967"]
["TECHNIK","VI  6-M10/PC",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M10 / šíře 18mm, izolace PC","100ks",17.81399957691751,{"$f":"F2183*(1-Elteq!$F$9)","v":17.81399957691751},"8591735055950"]
["TECHNIK","VI  6-M12",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M12 / šíře 21mm, izolace PVC","100ks",29.355986802795314,{"$f":"F2184*(1-Elteq!$F$9)","v":29.355986802795314},"8591735004033"]
["TECHNIK","VI  6-M16",null,"Vidlice izolovaná Cu, průřez 4,0-6,0mm2 / M16 / šíře 26mm, izolace PVC","100ks",30.84048676753844,{"$f":"F2185*(1-Elteq!$F$9)","v":30.84048676753844},"8591735004040"]
["TECHNIK","VI 10-M 4/PA",null,"Vidlice izolovaná Cu, průřez 10mm2 / M4 / šíře 10mm, izolace PA","100ks",28.205499330119391,{"$f":"F2186*(1-Elteq!$F$9)","v":28.205499330119391},"8591735002060"]
["TECHNIK","VI 10-M 5/PA",null,"Vidlice izolovaná Cu, průřez 10mm2 / M5 / šíře 10mm, izolace PA","100ks",29.318874303676736,{"$f":"F2187*(1-Elteq!$F$9)","v":29.318874303676736},"8591735009762"]
["TECHNIK","VI 10-M 6/PA",null,"Vidlice izolovaná Cu, průřez 10mm2 / M6 / šíře 11mm, izolace PA","100ks",32.658999224348769,{"$f":"F2188*(1-Elteq!$F$9)","v":32.658999224348769},"8591735009779"]
["TECHNIK","VI 10-M 8/PA",null,"Vidlice izolovaná Cu, průřez 10mm2 / M8 / šíře 14mm, izolace PA","100ks",33.40124920672033,{"$f":"F2189*(1-Elteq!$F$9)","v":33.40124920672033},"8591735009823"]
["TECHNIK","VI 10-M10/PA",null,"Vidlice izolovaná Cu, průřez 10mm2 / M10 / šíře 18mm, izolace PA","100ks",34.143499189091891,{"$f":"F2190*(1-Elteq!$F$9)","v":34.143499189091891},"8591735009830"]
["TECHNIK","VI 16-M 4/PA",null,"Vidlice izolovaná Cu, průřez 16mm2 / M4 / šíře 10mm, izolace PA","100ks",34.514624180277679,{"$f":"F2191*(1-Elteq!$F$9)","v":34.514624180277679},"8591735004057"]
["TECHNIK","VI 16-M 5/PA",null,"Vidlice izolovaná Cu, průřez 16mm2 / M5 / šíře 11mm, izolace PA","100ks",35.25687416264924,{"$f":"F2192*(1-Elteq!$F$9)","v":35.25687416264924},"8591735009854"]
["TECHNIK","VI 16-M 6/PA",null,"Vidlice izolovaná Cu, průřez 16mm2 / M6 / šíře 11mm, izolace PA","100ks",37.112499118578143,{"$f":"F2193*(1-Elteq!$F$9)","v":37.112499118578143},"8591735009793"]
["TECHNIK","VI 16-M 8/PA",null,"Vidlice izolovaná Cu, průřez 16mm2 / M8 / šíře 14mm, izolace PA","100ks",37.854749100949711,{"$f":"F2194*(1-Elteq!$F$9)","v":37.854749100949711},"8591735009755"]
["TECHNIK","VIF  1,5-M 4",null,"Vidlice izolovaná Cu zahnutá, průřez 0,5-1,5mm2 / M4 / šíře 8mm, izolace PVC","100ks",3.7112499118578146,{"$f":"F2195*(1-Elteq!$F$9)","v":3.7112499118578146},"8591735052072"]
["TECHNIK","VIF  1,5-M 5",null,"Vidlice izolovaná Cu zahnutá, průřez 0,5-1,5mm2 / M5 / šíře 10mm, izolace PVC","100ks",3.8968124074507053,{"$f":"F2196*(1-Elteq!$F$9)","v":3.8968124074507053},"8591735052089"]
["TECHNIK","VIF  2,5-M 4",null,"Vidlice izolovaná Cu zahnutá, průřez 1,5-2,5mm2 / M4 / šíře 8mm, izolace PVC","100ks",4.4906123933479556,{"$f":"F2197*(1-Elteq!$F$9)","v":4.4906123933479556},"8591735052096"]
["TECHNIK","VIF  2,5-M 5",null,"Vidlice izolovaná Cu zahnutá, průřez 1,5-2,5mm2 / M5 / šíře 10mm, izolace PVC","100ks",4.7132873880594248,{"$f":"F2198*(1-Elteq!$F$9)","v":4.7132873880594248},"8591735052102"]
["TECHNIK","VIF  6-M 4",null,"Vidlice izolovaná Cu zahnutá, průřez 4-6mm2 / M4 / šíře 8mm, izolace PVC","100ks",7.1627123298855819,{"$f":"F2199*(1-Elteq!$F$9)","v":7.1627123298855819},"8591735052119"]
["TECHNIK","VIF  6-M 5",null,"Vidlice izolovaná Cu zahnutá, průřez 4-6mm2 / M5 / šíře 10mm, izolace PVC","100ks",7.3482748254784731,{"$f":"F2200*(1-Elteq!$F$9)","v":7.3482748254784731},"8591735052126"]
["TECHNIK","VN  0,5-M 2",null,"Vidlice neizolovaná Cu, průřez 0,25-0,5mm2 / M2 / šíře 5mm","100ks",1.4473874656245478,{"$f":"F2201*(1-Elteq!$F$9)","v":1.4473874656245478},"8591735034054"]
["TECHNIK","VN  0,5-M 3",null,"Vidlice neizolovaná Cu, průřez 0,25-0,5mm2 / M3 / šíře 5mm","100ks",1.2247124709130788,{"$f":"F2202*(1-Elteq!$F$9)","v":1.2247124709130788},"8591735004064"]
["TECHNIK","VN  0,5-M 3,5",null,"Vidlice neizolovaná Cu, průřez 0,25-0,5mm2 / M3,5 / šíře 6mm","100ks",1.8927374550474854,{"$f":"F2203*(1-Elteq!$F$9)","v":1.8927374550474854},"8591735007775"]
["TECHNIK","VN  0,5-M 4",null,"Vidlice neizolovaná Cu, průřez 0,25-0,5mm2 / M4 / šíře 6,5mm","100ks",1.8927374550474854,{"$f":"F2204*(1-Elteq!$F$9)","v":1.8927374550474854},"8591735007898"]
["TECHNIK","VN  0,5-M 5",null,"Vidlice neizolovaná Cu, průřez 0,25-0,5mm2 / M5 / šíře 8mm","100ks",1.9669624532846417,{"$f":"F2205*(1-Elteq!$F$9)","v":1.9669624532846417},"8591735007867"]
["TECHNIK","VN  1,5-M 3",null,"Vidlice neizolovaná Cu, průřez 0,5-1,5mm2 / M3 / šíře 6mm","100ks",2.2267499471146888,{"$f":"F2206*(1-Elteq!$F$9)","v":2.2267499471146888},"8591735004071"]
["TECHNIK","VN  1,5-M 3,5",null,"Vidlice neizolovaná Cu, průřez 0,5-1,5mm2 / M3,5 / šíře 6mm","100ks",2.3009749453518449,{"$f":"F2207*(1-Elteq!$F$9)","v":2.3009749453518449},"8591735004088"]
["TECHNIK","VN  1,5-M 3,5/7",null,"Vidlice neizolovaná Cu, průřez 0,5-1,5mm2 / M3,5 / šíře 7,2mm","100ks",2.783437433893361,{"$f":"F2208*(1-Elteq!$F$9)","v":2.783437433893361},"8591735052133"]
["TECHNIK","VN  1,5-M 4",null,"Vidlice neizolovaná Cu, průřez 0,5-1,5mm2 / M4 / šíře 8mm","100ks",2.5607624391818922,{"$f":"F2209*(1-Elteq!$F$9)","v":2.5607624391818922},"8591735004095"]
["TECHNIK","VN  1,5-M 4/7",null,"Vidlice neizolovaná Cu, průřez 0,5-1,5mm2 / M4 / šíře 6,8mm","100ks",2.5607624391818922,{"$f":"F2210*(1-Elteq!$F$9)","v":2.5607624391818922},"8591735025496"]
["TECHNIK","VN  1,5-M 5",null,"Vidlice neizolovaná Cu, průřez 0,5-1,5mm2 / M5 / šíře 8mm","100ks",2.783437433893361,{"$f":"F2211*(1-Elteq!$F$9)","v":2.783437433893361},"8591735004101"]
["TECHNIK","VN  1,5-M 5/10",null,"Vidlice neizolovaná Cu, průřez 0,5-1,5mm2 / M5 / šíře 10mm","100ks",2.8576624321305171,{"$f":"F2212*(1-Elteq!$F$9)","v":2.8576624321305171},"8591735046057"]
["TECHNIK","VN  1,5-M 6",null,"Vidlice neizolovaná Cu, průřez 0,5-1,5mm2 / M6 / šíře 11mm","100ks",3.59991241450208,{"$f":"F2213*(1-Elteq!$F$9)","v":3.59991241450208},"8591735004118"]
["TECHNIK","VN  1,5-M 6/9",null,"Vidlice neizolovaná Cu, průřez 0,5-1,5mm2 / M6 / šíře 9,4mm","100ks",3.1545624250791424,{"$f":"F2214*(1-Elteq!$F$9)","v":3.1545624250791424},"8591735048440"]
["TECHNIK","VN  1,5-M 8",null,"Vidlice neizolovaná Cu, průřez 0,5-1,5mm2 / M8 / šíře 12mm","100ks",6.5689123439883321,{"$f":"F2215*(1-Elteq!$F$9)","v":6.5689123439883321},"8591735004125"]
["TECHNIK","VN  1,5-M10",null,"Vidlice neizolovaná Cu, průřez 0,5-1,5mm2 / M10 / šíře 17,5mm","100ks",10.688399746150505,{"$f":"F2216*(1-Elteq!$F$9)","v":10.688399746150505},"8591735004132"]
["TECHNIK","VN  1,5-M12",null,"Vidlice neizolovaná Cu, průřez 0,5-1,5mm2 / M12 / šíře 20mm","100ks",11.838887218826429,{"$f":"F2217*(1-Elteq!$F$9)","v":11.838887218826429},"8591735004149"]
["TECHNIK","VN  2,5-M 3",null,"Vidlice neizolovaná Cu, průřez 1,5-2,5mm2 / M3 / šíře 6mm","100ks",2.6720999365376263,{"$f":"F2218*(1-Elteq!$F$9)","v":2.6720999365376263},"8591735004156"]
["TECHNIK","VN  2,5-M 3,5",null,"Vidlice neizolovaná Cu, průřez 1,5-2,5mm2 / M3,5 / šíře 6mm","100ks",3.6370249136206585,{"$f":"F2219*(1-Elteq!$F$9)","v":3.6370249136206585},"8591735004163"]
["TECHNIK","VN  2,5-M 4",null,"Vidlice neizolovaná Cu, průřez 1,5-2,5mm2 / M4 / šíře 8mm","100ks",2.6720999365376263,{"$f":"F2220*(1-Elteq!$F$9)","v":2.6720999365376263},"8591735004170"]
["TECHNIK","VN  2,5-M 4/7",null,"Vidlice neizolovaná Cu, průřez 1,5-2,5mm2 / M4 / šíře 6,8mm","100ks",2.5236499400633141,{"$f":"F2221*(1-Elteq!$F$9)","v":2.5236499400633141},"8591735025489"]
["TECHNIK","VN  2,5-M 5",null,"Vidlice neizolovaná Cu, průřez 1,5-2,5mm2 / M5 / šíře 10mm","100ks",3.1916749241977205,{"$f":"F2222*(1-Elteq!$F$9)","v":3.1916749241977205},"8591735004187"]
["TECHNIK","VN  2,5-M 6",null,"Vidlice neizolovaná Cu, průřez 1,5-2,5mm2 / M6 / šíře 11mm","100ks",3.6741374127392366,{"$f":"F2223*(1-Elteq!$F$9)","v":3.6741374127392366},"8591735004194"]
["TECHNIK","VN  2,5-M 8",null,"Vidlice neizolovaná Cu, průřez 1,5-2,5mm2 / M8 / šíře 14mm","100ks",7.6080623193085195,{"$f":"F2224*(1-Elteq!$F$9)","v":7.6080623193085195},"8591735004200"]
["TECHNIK","VN  2,5-M10",null,"Vidlice neizolovaná Cu, průřez 1,5-2,5mm2 / M10 / šíře 17,5mm","100ks",10.688399746150505,{"$f":"F2225*(1-Elteq!$F$9)","v":10.688399746150505},"8591735004217"]
["TECHNIK","VN  2,5-M12",null,"Vidlice neizolovaná Cu, průřez 1,5-2,5mm2 / M12 / šíře 20mm","100ks",11.950224716182163,{"$f":"F2226*(1-Elteq!$F$9)","v":11.950224716182163},"8591735004224"]
["TECHNIK","VN  6-M 3,5",null,"Vidlice neizolovaná Cu, průřez 4-6mm2 / M3,5 / šíře 6,4mm","100ks",4.3421623968736434,{"$f":"F2227*(1-Elteq!$F$9)","v":4.3421623968736434},"8591735011086"]
["TECHNIK","VN  6-M 4",null,"Vidlice neizolovaná Cu, průřez 4-6mm2 / M4 / šíře 8mm","100ks",4.3421623968736434,{"$f":"F2228*(1-Elteq!$F$9)","v":4.3421623968736434},"8591735004231"]
["TECHNIK","VN  6-M 5",null,"Vidlice neizolovaná Cu, průřez 4-6mm2 / M5 / šíře 10mm","100ks",5.1586373774823624,{"$f":"F2229*(1-Elteq!$F$9)","v":5.1586373774823624},"8591735004248"]
["TECHNIK","VN  6-M 6",null,"Vidlice neizolovaná Cu, průřez 4-6mm2 / M6 / šíře 13,5mm","100ks",5.3813123721938307,{"$f":"F2230*(1-Elteq!$F$9)","v":5.3813123721938307},"8591735004255"]
["TECHNIK","VN  6-M 8",null,"Vidlice neizolovaná Cu, průřez 4-6mm2 / M8 / šíře 14mm","100ks",8.869887289340177,{"$f":"F2231*(1-Elteq!$F$9)","v":8.869887289340177},"8591735004262"]
["TECHNIK","VN  6-M10",null,"Vidlice neizolovaná Cu, průřez 4-6mm2 / M10 / šíře 18mm","100ks",12.098674712656475,{"$f":"F2232*(1-Elteq!$F$9)","v":12.098674712656475},"8591735004279"]
["TECHNIK","VN  6-M12",null,"Vidlice neizolovaná Cu, průřez 4-6mm2 / M12 / šíře 21mm","100ks",18.630474557526231,{"$f":"F2233*(1-Elteq!$F$9)","v":18.630474557526231},"8591735004286"]
["TECHNIK","VN  6-M16",null,"Vidlice neizolovaná Cu, průřez 4-6mm2 / M16 / šíře 26mm","100ks",22.527286964976934,{"$f":"F2234*(1-Elteq!$F$9)","v":22.527286964976934},"8591735004293"]
["TECHNIK","VN 10-M 4",null,"Vidlice neizolovaná Cu, průřez 10mm2 / M4 / šíře 10mm","100ks",10.020374762016099,{"$f":"F2235*(1-Elteq!$F$9)","v":10.020374762016099},"8591735004309"]
["TECHNIK","VN 10-M 5",null,"Vidlice neizolovaná Cu, průřez 10mm2 / M5 / šíře 10mm","100ks",9.8348122664232083,{"$f":"F2236*(1-Elteq!$F$9)","v":9.8348122664232083},"8591735004316"]
["TECHNIK","VN 10-M 6",null,"Vidlice neizolovaná Cu, průřez 10mm2 / M6 / šíře 11mm","100ks",8.5729872963915525,{"$f":"F2237*(1-Elteq!$F$9)","v":8.5729872963915525},"8591735004323"]
["TECHNIK","VN 10-M 8",null,"Vidlice neizolovaná Cu, průřez 10mm2 / M8 / šíře 14mm","100ks",25.42206189622603,{"$f":"F2238*(1-Elteq!$F$9)","v":25.42206189622603},"8591735007843"]
["TECHNIK","VN 10-M10",null,"Vidlice neizolovaná Cu, průřez 10mm2 / M10 / šíře 18mm","100ks",30.098236785166876,{"$f":"F2239*(1-Elteq!$F$9)","v":30.098236785166876},"8591735008000"]
["TECHNIK","VN 16-M 5",null,"Vidlice neizolovaná Cu, průřez 16mm2 / M5 / šíře 11mm","100ks",30.246686781641188,{"$f":"F2240*(1-Elteq!$F$9)","v":30.246686781641188},"8591735010478"]
["TECHNIK","VN 16-M 6",null,"Vidlice neizolovaná Cu, průřez 16mm2 / M6 / šíře 11mm","100ks",30.246686781641188,{"$f":"F2241*(1-Elteq!$F$9)","v":30.246686781641188},"8591735004330"]
["TECHNIK","VN 16-M 8",null,"Vidlice neizolovaná Cu, průřez 16mm2 / M8 / šíře 14mm","100ks",32.287874233162988,{"$f":"F2242*(1-Elteq!$F$9)","v":32.287874233162988},"8591735004347"]
["TECHNIK","VN 16-M10",null,"Vidlice neizolovaná Cu, průřez 16mm2 / M10 / šíře 18mm","100ks",35.071311667056349,{"$f":"F2243*(1-Elteq!$F$9)","v":35.071311667056349},"8591735010461"]
["TECHNIK","VIS 1,5-M 3",null,"Vidlice lisovací Cu se smrštitelnou bužírkou, průřez 0,5-1,5mm2 / M3 / 6mm","100ks",14.102749665059696,{"$f":"F2244*(1-Elteq!$F$9)","v":14.102749665059696},"8591735026400"]
["TECHNIK","VIS 1,5-M 3,5",null,"Vidlice lisovací Cu se smrštitelnou bužírkou, průřez 0,5-1,5mm2 / M3,5 / 6,4mm","100ks",14.102749665059696,{"$f":"F2245*(1-Elteq!$F$9)","v":14.102749665059696},"8591735026745"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"VIS 1,5-M 4",null,"Vidlice lisovací Cu se smrštitelnou bužírkou, průřez 0,5-1,5mm2 / M4 / 8mm","100ks",14.102749665059696,{"$f":"F2246*(1-Elteq!$F$9)","v":14.102749665059696},"8591735026752"]
["TECHNIK","VIS 1,5-M 4/7",null,"Vidlice lisovací Cu se smrštitelnou bužírkou, průřez 0,5-1,5mm2 / M4 / 6,8mm","100ks",14.102749665059696,{"$f":"F2247*(1-Elteq!$F$9)","v":14.102749665059696},"8591735026769"]
["TECHNIK","VIS 1,5-M 5",null,"Vidlice lisovací Cu se smrštitelnou bužírkou, průřez 0,5-1,5mm2 / M5 / 8mm","100ks",14.102749665059696,{"$f":"F2248*(1-Elteq!$F$9)","v":14.102749665059696},"8591735026776"]
["TECHNIK","VIS 1,5-M 6",null,"Vidlice lisovací Cu se smrštovací bužírkou, průřez 0,5-1,5mm2 / M6 / 11mm","100ks",15.587249629802821,{"$f":"F2249*(1-Elteq!$F$9)","v":15.587249629802821},"8591735026783"]
["TECHNIK","VIS 2,5-M 3",null,"Vidlice lisovací Cu se smrštovací bužírkou, průřez 1,5-2,5mm2 / M3 / 6mm","100ks",14.102749665059696,{"$f":"F2250*(1-Elteq!$F$9)","v":14.102749665059696},"8591735026790"]
["TECHNIK","VIS 2,5-M 3,5",null,"Vidlice lisovací Cu se smrštovací bužírkou, průřez 1,5-2,5mm2 / M3,5 / 6,4mm","100ks",14.102749665059696,{"$f":"F2251*(1-Elteq!$F$9)","v":14.102749665059696},"8591735026806"]
["TECHNIK","VIS 2,5-M 4",null,"Vidlice lisovací Cu se smrštovací bužírkou, průřez 1,5-2,5mm2 / M4 / 8mm","100ks",14.102749665059696,{"$f":"F2252*(1-Elteq!$F$9)","v":14.102749665059696},"8591735026813"]
["TECHNIK","VIS 2,5-M 4/7",null,"Vidlice lisovací Cu se smrštovací bužírkou, průřez 1,5-2,5mm2 / M4 / 6,8mm","100ks",14.102749665059696,{"$f":"F2253*(1-Elteq!$F$9)","v":14.102749665059696},"8591735026820"]
["TECHNIK","VIS 2,5-M 5",null,"Vidlice lisovací Cu se smrštovací bužírkou, průřez 1,5-2,5mm2 / M5 / 10mm","100ks",14.102749665059696,{"$f":"F2254*(1-Elteq!$F$9)","v":14.102749665059696},"8591735026837"]
["TECHNIK","VIS 2,5-M 5/8",null,"Vidlice lisovací Cu se smrštovací bužírkou, průřez 1,5-2,5mm2 / M5 / 8,5mm","100ks",14.102749665059696,{"$f":"F2255*(1-Elteq!$F$9)","v":14.102749665059696},"8591735026844"]
["TECHNIK","VIS 2,5-M 6",null,"Vidlice lisovací Cu se smrštovací bužírkou, průřez 1,5-2,5mm2 / M6 / 11mm","100ks",15.587249629802821,{"$f":"F2256*(1-Elteq!$F$9)","v":15.587249629802821},"8591735026851"]
["TECHNIK","VIS 6-M 3",null,"Vidlice lisovací Cu se smrštovací bužírkou, průřez 4-6mm2 / M3 / 5,8mm","100ks",19.669624532846417,{"$f":"F2257*(1-Elteq!$F$9)","v":19.669624532846417},"8591735026868"]
["TECHNIK","VIS 6-M 3,5",null,"Vidlice lisovací Cu se smrštovací bužírkou, průřez 4-6mm2 / M3,5 / 6,4mm","100ks",19.669624532846417,{"$f":"F2258*(1-Elteq!$F$9)","v":19.669624532846417},"8591735026875"]
["TECHNIK","VIS 6-M 4",null,"Vidlice lisovací Cu se smrštovací bužírkou, průřez 4-6mm2 / M4 / šíře 8mm","100ks",19.669624532846417,{"$f":"F2259*(1-Elteq!$F$9)","v":19.669624532846417},"8591735026882"]
["TECHNIK","VIS 6-M 5",null,"Vidlice lisovací Cu se smrštovací bužírkou, průřez 4-6mm2 / M5 / 10mm","100ks",19.669624532846417,{"$f":"F2260*(1-Elteq!$F$9)","v":19.669624532846417},"8591735026899"]
["TECHNIK","VIS 6-M 6",null,"Vidlice lisovací Cu se smrštovací bužírkou, průřez 4-6mm2 / M6 / 12mm","100ks",21.896374479961107,{"$f":"F2261*(1-Elteq!$F$9)","v":21.896374479961107},"8591735026905"]
["TECHNIK","VIS 6-M 8",null,"Vidlice lisovací Cu se smrštovací bužírkou, průřez 4-6mm2 / M8 / 14mm","100ks",21.896374479961107,{"$f":"F2262*(1-Elteq!$F$9)","v":21.896374479961107},"8591735026912"]
["TECHNIK","VIS 6-M10",null,"Vidlice lisovací Cu se smrštovací bužírkou, průřez 4-6mm2 / M10 / 18mm","100ks",25.050936905040249,{"$f":"F2263*(1-Elteq!$F$9)","v":25.050936905040249},"8591735026929"]
["TECHNIK","PB 2,0 bílá",null,"Popisovací bužírka PVC, vnitřní průměr 2,0mm bílá BA-20 pro tiskárny bužírek (cívka 200m)","200m",43.792748959922214,{"$f":"F2264*(1-Elteq!$F$9)","v":43.792748959922214},"8591735020668"]
["TECHNIK","PB 2,0 žlutá",null,"Popisovací bužírka PVC, vnitřní průměr 2,0mm žlutá BA20Z pro tiskárny bužírek (cívka 200m)","200m",50.472998801266279,{"$f":"F2265*(1-Elteq!$F$9)","v":50.472998801266279},"8591735020675"]
["TECHNIK","PB 2,5 bílá",null,"Popisovací bužírka PVC, vnitřní průměr 2,5mm bílá BA-25 pro tiskárny bužírek (cívka 200m)","200m",43.792748959922214,{"$f":"F2266*(1-Elteq!$F$9)","v":43.792748959922214},"8591735020682"]
["TECHNIK","PB 2,5 žlutá",null,"Popisovací bužírka PVC, vnitřní průměr 2,5mm žlutá BA25Z pro tiskárny bužírek (cívka 200m)","200m",50.472998801266279,{"$f":"F2267*(1-Elteq!$F$9)","v":50.472998801266279},"8591735020699"]
["TECHNIK","PB 3,0 bílá",null,"Popisovací bužírka PVC, vnitřní průměr 3,0mm bílá BA-30 pro tiskárny bužírek (cívka 200m)","200m",48.988498836523149,{"$f":"F2268*(1-Elteq!$F$9)","v":48.988498836523149},"8591735020705"]
["TECHNIK","PB 3,0 žlutá",null,"Popisovací bužírka PVC, vnitřní průměr 3,0mm žlutá BA30Z pro tiskárny bužírek (cívka 200m)","200m",57.895498624981904,{"$f":"F2269*(1-Elteq!$F$9)","v":57.895498624981904},"8591735020712"]
["TECHNIK","PB 3,2 žlutá",null,"Popisovací bužírka PVC, vnitřní průměr 3,2mm žlutá BA32Z pro tiskárny bužírek (cívka 200m)","200m",61.606748536839724,{"$f":"F2270*(1-Elteq!$F$9)","v":61.606748536839724},"8591735047764"]
["TECHNIK","PB 3,5 bílá",null,"Popisovací bužírka PVC, vnitřní průměr 3,5mm bílá BA-35 pro tiskárny bužírek (cívka 200m)","200m",57.895498624981904,{"$f":"F2271*(1-Elteq!$F$9)","v":57.895498624981904},"8591735020729"]
["TECHNIK","PB 3,5 žlutá",null,"Popisovací bužírka PVC, vnitřní průměr 3,5mm žlutá BA35Z pro tiskárny bužírek (cívka 200m)","200m",63.833498483954408,{"$f":"F2272*(1-Elteq!$F$9)","v":63.833498483954408},"8591735020736"]
["TECHNIK","PB 4,0 bílá",null,"Popisovací bužírka PVC, vnitřní průměr 4,0mm bílá BA-40 pro tiskárny bužírek (cívka 200m)","200m",64.575748466325976,{"$f":"F2273*(1-Elteq!$F$9)","v":64.575748466325976},"8591735020743"]
["TECHNIK","PB 4,0 žlutá",null,"Popisovací bužírka PVC, vnitřní průměr 4,0mm žlutá BA40Z pro tiskárny bužírek (cívka 200m)","200m",75.709498201899422,{"$f":"F2274*(1-Elteq!$F$9)","v":75.709498201899422},"8591735020750"]
["TECHNIK","PB 4,5 bílá",null,"Popisovací bužírka PVC, vnitřní průměr 4,5mm bílá BA-45 pro tiskárny bužírek (cívka 200m)","200m",77.193998166642544,{"$f":"F2275*(1-Elteq!$F$9)","v":77.193998166642544},"8591735020767"]
["TECHNIK","PB 4,5 žlutá",null,"Popisovací bužírka PVC, vnitřní průměr 4,5mm žlutá BA45Z pro tiskárny bužírek (cívka 200m)","200m",92.781247796445371,{"$f":"F2276*(1-Elteq!$F$9)","v":92.781247796445371},"8591735020774"]
["TECHNIK","PB 5,0 bílá",null,"Popisovací bužírka PVC, vnitřní průměr 5,0mm bílá BA-50 pro tiskárny bužírek (cívka 200m)","200m",84.61649799035817,{"$f":"F2277*(1-Elteq!$F$9)","v":84.61649799035817},"8591735020781"]
["TECHNIK","PB 5,0 žlutá",null,"Popisovací bužírka PVC, vnitřní průměr 5,0mm žlutá BA50Z pro tiskárny bužírek (cívka 200m)","200m",101.68824758490412,{"$f":"F2278*(1-Elteq!$F$9)","v":101.68824758490412},"8591735020798"]
["TECHNIK","PB 5,5 bílá",null,"Popisovací bužírka PVC, vnitřní průměr 5,5mm bílá BA-55 pro tiskárny bužírek (cívka 200m)","200m",94.265747761188493,{"$f":"F2279*(1-Elteq!$F$9)","v":94.265747761188493},"8591735020804"]
["TECHNIK","PB 5,5 žlutá",null,"Popisovací bužírka PVC, vnitřní průměr 5,5mm žlutá BA55Z pro tiskárny bužírek (cívka 200m)","200m",111.33749735573444,{"$f":"F2280*(1-Elteq!$F$9)","v":111.33749735573444},"8591735020811"]
["TECHNIK","PB 6,0 bílá",null,"Popisovací bužírka PVC, vnitřní průměr 6,0mm bílá BA-60 pro tiskárny bužírek (cívka 200m)","200m",103.9149975320188,{"$f":"F2281*(1-Elteq!$F$9)","v":103.9149975320188},"8591735020828"]
["TECHNIK","PB 6,0 žlutá",null,"Popisovací bužírka PVC, vnitřní průměr 6,0mm žlutá BA60Z pro tiskárny bužírek (cívka 200m)","200m",118.75999717945007,{"$f":"F2282*(1-Elteq!$F$9)","v":118.75999717945007},"8591735020835"]
["TECHNIK","PB 8,0 bílá",null,"Popisovací bužírka PVC, vnitřní průměr 8,0mm bílá BA-80 pro tiskárny bužírek (cívka 100m)","100m",76.822873175456763,{"$f":"F2283*(1-Elteq!$F$9)","v":76.822873175456763},"8591735020842"]
["TECHNIK","PB 8,0 žlutá",null,"Popisovací bužírka PVC, vnitřní průměr 8,0mm žlutá BA80Z pro tiskárny bužírek (cívka 100m)","100m",92.781247796445371,{"$f":"F2284*(1-Elteq!$F$9)","v":92.781247796445371},"8591735020859"]
["TECHNIK","PB10,0 bílá",null,"Popisovací bužírka PVC, vnitřní průměr 10,0mm bílá BA-100 pro tiskárny bužírek (cívka 100m)","100m",86.843247937472867,{"$f":"F2285*(1-Elteq!$F$9)","v":86.843247937472867},"8591735020866"]
["TECHNIK","PB10,0 žlutá",null,"Popisovací bužírka PVC, vnitřní průměr 10,0mm žlutá BA100Z pro tiskárny bužírek (cívka 100m)","100m",99.832622628975216,{"$f":"F2286*(1-Elteq!$F$9)","v":99.832622628975216},"8591735020873"]
["TECHNIK","PKZ 2/6",null,"Navlékací profil pro držák PKH, délka 6mm, bez potisku, žlutá","500ks",28.205499330119391,{"$f":"F2287*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"-\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"-\", žlutá","500ks",28.205499330119391,{"$f":"F2288*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \".\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \".\", žlutá","500ks",28.205499330119391,{"$f":"F2289*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"0\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"0\", žlutá","500ks",28.205499330119391,{"$f":"F2290*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"1\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"1\", žlutá","500ks",28.205499330119391,{"$f":"F2291*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"2\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"2\", žlutá","500ks",28.205499330119391,{"$f":"F2292*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"3\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"3\", žlutá","500ks",28.205499330119391,{"$f":"F2293*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"4\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"4\", žlutá","500ks",28.205499330119391,{"$f":"F2294*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"5\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"5\", žlutá","500ks",28.205499330119391,{"$f":"F2295*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"6\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"6\", žlutá","500ks",28.205499330119391,{"$f":"F2296*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"7\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"7\", žlutá","500ks",28.205499330119391,{"$f":"F2297*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"8\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"8\", žlutá","500ks",28.205499330119391,{"$f":"F2298*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"9\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"9\", žlutá","500ks",28.205499330119391,{"$f":"F2299*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"A\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"A\", žlutá","500ks",28.205499330119391,{"$f":"F2300*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"B\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"B\", žlutá","500ks",28.205499330119391,{"$f":"F2301*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"C\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"C\", žlutá","500ks",28.205499330119391,{"$f":"F2302*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"D\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"D\", žlutá","500ks",28.205499330119391,{"$f":"F2303*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"E\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"E\", žlutá","500ks",28.205499330119391,{"$f":"F2304*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"F\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"F\", žlutá","500ks",28.205499330119391,{"$f":"F2305*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"G\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"G\", žlutá","500ks",28.205499330119391,{"$f":"F2306*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"H\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"H\", žlutá","500ks",28.205499330119391,{"$f":"F2307*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"K\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"K\", žlutá","500ks",28.205499330119391,{"$f":"F2308*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"L\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"L\", žlutá","500ks",28.205499330119391,{"$f":"F2309*(1-Elteq!$F$9)","v":28.205499330119391},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"PKZ 2/6 \"M\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"M\", žlutá","500ks",28.205499330119391,{"$f":"F2310*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"N\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"N\", žlutá","500ks",28.205499330119391,{"$f":"F2311*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"O\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"O\", žlutá","500ks",28.205499330119391,{"$f":"F2312*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"P\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"P\", žlutá","500ks",28.205499330119391,{"$f":"F2313*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"R\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"R\", žlutá","500ks",28.205499330119391,{"$f":"F2314*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"S\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"S\", žlutá","500ks",28.205499330119391,{"$f":"F2315*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"T\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"T\", žlutá","500ks",28.205499330119391,{"$f":"F2316*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"U\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"U\", žlutá","500ks",28.205499330119391,{"$f":"F2317*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"V\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"V\", žlutá","500ks",28.205499330119391,{"$f":"F2318*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"W\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"W\", žlutá","500ks",28.205499330119391,{"$f":"F2319*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"X\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"X\", žlutá","500ks",28.205499330119391,{"$f":"F2320*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"Y\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"Y\", žlutá","500ks",28.205499330119391,{"$f":"F2321*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","PKZ 2/6 \"Z\"",null,"Navlékací profil pro držák PKH, délka 6mm, s potiskem \"Z\", žlutá","500ks",28.205499330119391,{"$f":"F2322*(1-Elteq!$F$9)","v":28.205499330119391},""]
["TECHNIK","EDH 265",null,"Elektrikářský drátovací hřeben rozměr 265x32x14mm, PE bralen bezhalogenový","50ks",34.514624180277679,{"$f":"F2323*(1-Elteq!$F$9)","v":34.514624180277679},"8591735047108"]
["TECHNIK","KAOB  3",null,"Kabelová objímka přírodní plastová Polyamid 66 pro průměr kabelu 3,2 mm","100ks",2.8947749312490956,{"$f":"F2324*(1-Elteq!$F$9)","v":2.8947749312490956},"8591735009199"]
["TECHNIK","KAOB  5",null,"Kabelová objímka přírodní plastová Polyamid 66 pro průměr kabelu 4,8 mm","100ks",2.9689999294862517,{"$f":"F2325*(1-Elteq!$F$9)","v":2.9689999294862517},"8591735009205"]
["TECHNIK","KAOB  6",null,"Kabelová objímka přírodní plastová Polyamid 66 pro průměr kabelu 6,3 mm","100ks",3.1545624250791424,{"$f":"F2326*(1-Elteq!$F$9)","v":3.1545624250791424},"8591735009212"]
["TECHNIK","KAOB  8",null,"Kabelová objímka přírodní plastová Polyamid 66 pro průměr kabelu 7,9 mm","100ks",3.4514624180277678,{"$f":"F2327*(1-Elteq!$F$9)","v":3.4514624180277678},"8591735009229"]
["TECHNIK","KAOB 10",null,"Kabelová objímka přírodní plastová Polyamid 66 pro průměr kabelu 9,5 mm","100ks",3.6370249136206585,{"$f":"F2328*(1-Elteq!$F$9)","v":3.6370249136206585},"8591735009236"]
["TECHNIK","KAOB 13",null,"Kabelová objímka přírodní plastová Polyamid 66 pro průměr kabelu 12,7 mm","100ks",4.7875123862965809,{"$f":"F2329*(1-Elteq!$F$9)","v":4.7875123862965809},"8591735009243"]
["TECHNIK","KAOB 16",null,"Kabelová objímka přírodní plastová Polyamid 66 pro průměr kabelu 15,8 mm","100ks",5.2328623757195185,{"$f":"F2330*(1-Elteq!$F$9)","v":5.2328623757195185},"8591735009250"]
["TECHNIK","KAOB 19",null,"Kabelová objímka přírodní plastová Polyamid 66 pro průměr kabelu 19,4 mm","100ks",7.1627123298855819,{"$f":"F2331*(1-Elteq!$F$9)","v":7.1627123298855819},"8591735009267"]
["TECHNIK","KAOB 25",null,"Kabelová objímka přírodní plastová Polyamid 66 pro průměr kabelu 25,4 mm","100ks",7.979187310494301,{"$f":"F2332*(1-Elteq!$F$9)","v":7.979187310494301},"8591735049690"]
["TECHNIK","KAOB 28",null,"Kabelová objímka přírodní plastová Polyamid 66 pro průměr kabelu 27,5 mm","100ks",8.7956622911030209,{"$f":"F2333*(1-Elteq!$F$9)","v":8.7956622911030209},"8591735009274"]
["TECHNIK","KAOB 37",null,"Kabelová objímka přírodní plastová Polyamid 66 pro průměr kabelu 36,7 mm","100ks",11.096637236454866,{"$f":"F2334*(1-Elteq!$F$9)","v":11.096637236454866},"8591735009281"]
["TECHNIK","KAOBC  3",null,"Kabelová objímka černá plastová Polyamid 66 pro průměr kabelu 3,2 mm","100ks",3.1916749241977205,{"$f":"F2335*(1-Elteq!$F$9)","v":3.1916749241977205},"8591735051662"]
["TECHNIK","KAOBC  6",null,"Kabelová objímka černá plastová Polyamid 66 pro průměr kabelu 6,3 mm","100ks",3.4885749171463458,{"$f":"F2336*(1-Elteq!$F$9)","v":3.4885749171463458},"8591735050894"]
["TECHNIK","KAOBC  7",null,"Kabelová objímka černá plastová Polyamid 66 pro průměr kabelu 7,2 mm / otvor pro šroub 4,4mm","100ks",3.7854749100949707,{"$f":"F2337*(1-Elteq!$F$9)","v":3.7854749100949707},"8591735052492"]
["TECHNIK","KAOBC  8",null,"Kabelová objímka černá plastová Polyamid 66 pro průměr kabelu 7,9 mm / otvor pro šroub 5,2mm","100ks",9.2038997814073795,{"$f":"F2338*(1-Elteq!$F$9)","v":9.2038997814073795},"8591735052485"]
["TECHNIK","KAOBC 10",null,"Kabelová objímka černá plastová Polyamid 66 pro průměr kabelu 10,0 mm","100ks",4.00814990480644,{"$f":"F2339*(1-Elteq!$F$9)","v":4.00814990480644},"8591735051679"]
["TECHNIK","KAOBC 28",null,"Kabelová objímka černá plastová Polyamid 66 pro průměr kabelu 27,5 mm rozměry 4,6x12x50x1,8mm","100ks",12.024449714419319,{"$f":"F2340*(1-Elteq!$F$9)","v":12.024449714419319},"8591735056483"]
["TECHNIK","KAOBF  8",null,"Kabelová příchytka jednostranná kovová pro průměr kabelu 8,0mm / upevňovací otvor průměr 5,5mm","100ks",13.471837180043867,{"$f":"F2341*(1-Elteq!$F$9)","v":13.471837180043867},"8591735049904"]
["TECHNIK","KAOBFE 1204",null,"Kabelová objímka ocelová potažená gumou pro průměr kabelu 4,0mm / šíře 12mm / otvor 5,3mm","100ks",15.216124638617039,{"$f":"F2342*(1-Elteq!$F$9)","v":15.216124638617039},"8591735055141"]
["TECHNIK","KAOBFE 1205",null,"Kabelová objímka ocelová potažená gumou pro průměr kabelu 5,0mm / šíře 12mm / otvor 5,3mm","100ks",15.290349636854197,{"$f":"F2343*(1-Elteq!$F$9)","v":15.290349636854197},"8591735054038"]
["TECHNIK","KAOBFE 1206",null,"Kabelová objímka ocelová potažená gumou pro průměr kabelu 6,0mm / šíře 12mm / otvor 5,3mm","100ks",15.99548712010718,{"$f":"F2344*(1-Elteq!$F$9)","v":15.99548712010718},"8591735055158"]
["TECHNIK","KAOBFE 1206 N",null,"Kabelová objímka nerezová potažená gumou pro průměr kabelu 6,4mm / šíře 12,7mm / otvor 7,0mm","100ks",36.036236644139379,{"$f":"F2345*(1-Elteq!$F$9)","v":36.036236644139379},"8591735053215"]
["TECHNIK","KAOBFE 1208",null,"Kabelová objímka ocelová potažená gumou pro průměr kabelu 8,0mm / šíře 12mm / otvor 5,3mm","100ks",16.700624603360165,{"$f":"F2346*(1-Elteq!$F$9)","v":16.700624603360165},"8591735049911"]
["TECHNIK","KAOBFE 1210",null,"Kabelová objímka ocelová potažená gumou pro průměr kabelu 10,0mm / šíře 12mm / otvor 5,3mm","100ks",17.776887077798932,{"$f":"F2347*(1-Elteq!$F$9)","v":17.776887077798932},"8591735055868"]
["TECHNIK","KAOBFE 1210 N",null,"Kabelová objímka nerezová potažená gumou pro průměr kabelu 9,5mm / šíře 12,7mm / otvor 7,0mm","100ks",40.935086527791697,{"$f":"F2348*(1-Elteq!$F$9)","v":40.935086527791697},"8591735053222"]
["TECHNIK","KAOBFE 1212",null,"Kabelová objímka ocelová potažená gumou pro průměr kabelu 12,0mm / šíře 12mm / otvor 5,3mm","100ks",18.816037053119121,{"$f":"F2349*(1-Elteq!$F$9)","v":18.816037053119121},"8591735049935"]
["TECHNIK","KAOBFE 1214",null,"Kabelová objímka ocelová potažená gumou pro průměr kabelu 14,0mm / šíře 12mm / otvor 5,3mm","100ks",19.966524525795041,{"$f":"F2350*(1-Elteq!$F$9)","v":19.966524525795041},"8591735049942"]
["TECHNIK","KAOBFE 1214 N",null,"Kabelová objímka nerezová potažená gumou pro průměr kabelu 14,3mm / šíře 12,7mm / otvor 7,0mm","100ks",45.648373915851117,{"$f":"F2351*(1-Elteq!$F$9)","v":45.648373915851117},"8591735057008"]
["TECHNIK","KAOBFE 1216",null,"Kabelová objímka ocelová potažená gumou pro průměr kabelu 16,0mm / šíře 12mm / otvor 5,3mm","100ks",21.00567450111523,{"$f":"F2352*(1-Elteq!$F$9)","v":21.00567450111523},"8591735051549"]
["TECHNIK","KAOBFE 1219",null,"Kabelová objímka ocelová potažená gumou pro průměr kabelu 19,0mm / šíře 12mm / otvor 5,3mm","100ks",21.785036982605373,{"$f":"F2353*(1-Elteq!$F$9)","v":21.785036982605373},"8591735049928"]
["TECHNIK","KAOBFE 1532",null,"Kabelová objímka ocelová potažená gumou pro průměr kabelu 32,0mm / šíře 15mm / otvor 6,3mm","50ks",23.009749453518449,{"$f":"F2354*(1-Elteq!$F$9)","v":23.009749453518449},"8591735055066"]
["TECHNIK","KAOBFE 1538",null,"Kabelová objímka ocelová potažená gumou pro průměr kabelu 38,0mm / šíře 15mm / otvor 6,3mm","50ks",24.939599407684515,{"$f":"F2355*(1-Elteq!$F$9)","v":24.939599407684515},"8591735052270"]
["TECHNIK","KAOH  3,5",null,"Kabelová objímka bílá s hřebíkem pro průměr 3,5 mm","100ks",1.4102749665059695,{"$f":"F2356*(1-Elteq!$F$9)","v":1.4102749665059695},"8591735036560"]
["TECHNIK","KAOH  5",null,"Kabelová objímka bílá s hřebíkem pro průměr 5 mm","100ks",1.5216124638617039,{"$f":"F2357*(1-Elteq!$F$9)","v":1.5216124638617039},"8591735009083"]
["TECHNIK","KAOH  5 šedá",null,"Kabelová objímka šedá s hřebíkem pro průměr 5 mm","100ks",1.7071749594545946,{"$f":"F2358*(1-Elteq!$F$9)","v":1.7071749594545946},"8591735014469"]
["TECHNIK","KAOH  7",null,"Kabelová objímka bílá s hřebíkem pro průměr 7 mm","100ks",1.9669624532846417,{"$f":"F2359*(1-Elteq!$F$9)","v":1.9669624532846417},"8591735009090"]
["TECHNIK","KAOH  7 šedá",null,"Kabelová objímka šedá s hřebíkem pro průměr 7 mm","100ks",2.1525249488775327,{"$f":"F2360*(1-Elteq!$F$9)","v":2.1525249488775327},"8591735014476"]
["TECHNIK","KAOH  9",null,"Kabelová objímka bílá s hřebíkem pro průměr 9 mm","100ks",2.4494249418261576,{"$f":"F2361*(1-Elteq!$F$9)","v":2.4494249418261576},"8591735009106"]
["TECHNIK","KAOH  9 šedá",null,"Kabelová objímka šedá s hřebíkem pro průměr 9 mm","100ks",2.7092124356562048,{"$f":"F2362*(1-Elteq!$F$9)","v":2.7092124356562048},"8591735014391"]
["TECHNIK","KAOH 11",null,"Kabelová objímka bílá s hřebíkem pro průměr 11 mm","100ks",2.9689999294862517,{"$f":"F2363*(1-Elteq!$F$9)","v":2.9689999294862517},"8591735009113"]
["TECHNIK","KAOH 11 šedá",null,"Kabelová objímka šedá s hřebíkem pro průměr 11 mm","100ks",3.3030124215534551,{"$f":"F2364*(1-Elteq!$F$9)","v":3.3030124215534551},"8591735014483"]
["TECHNIK","KAOH 14",null,"Kabelová objímka s hřebíkem pro průměr 14 mm","100ks",3.4885749171463458,{"$f":"F2365*(1-Elteq!$F$9)","v":3.4885749171463458},"8591735013028"]
["TECHNIK","KAOH 18",null,"Kabelová objímka s hřebíkem pro průměr 18 mm","100ks",4.3421623968736434,{"$f":"F2366*(1-Elteq!$F$9)","v":4.3421623968736434},"8591735013035"]
["TECHNIK","KAOH 6/2",null,"Kabelová objímka s hřebíkem pro dvoilinku 6,2x3,8 mm","100ks",1.5216124638617039,{"$f":"F2367*(1-Elteq!$F$9)","v":1.5216124638617039},"8591735009120"]
["TECHNIK","KAOH10/2",null,"Kabelová objímka s hřebíkem pro dvoulinku 10,0x6,5 mm","100ks",2.041187451521798,{"$f":"F2368*(1-Elteq!$F$9)","v":2.041187451521798},"8591735009137"]
["TECHNIK","KAS 10",null,"Kabelová samolepicí spona pro svazek 7-10mm / základna 17,4x17,4mm","100ks",14.696549650956946,{"$f":"F2369*(1-Elteq!$F$9)","v":14.696549650956946},"8591735013417"]
["TECHNIK","KAS 15",null,"Kabelová samolepicí spona pro svazek 10-15mm / základna 22,0x22,0mm","100ks",19.59539953460926,{"$f":"F2370*(1-Elteq!$F$9)","v":19.59539953460926},"8591735013424"]
["TECHNIK","KAS 20",null,"Kabelová samolepicí spona pro svazek 15-20mm / základna 25,5x25,5mm","100ks",20.040749524032197,{"$f":"F2371*(1-Elteq!$F$9)","v":20.040749524032197},"8591735013431"]
["TECHNIK","KS  5",null,"Kabelová spona přírodní plastová pro svazek o průměru 4-7mm","100ks",2.783437433893361,{"$f":"F2372*(1-Elteq!$F$9)","v":2.783437433893361},"8591735025045"]
["TECHNIK","KS  8",null,"Kabelová spona přírodní plastová pro svazek o průměru 7-10mm","100ks",2.9318874303676736,{"$f":"F2373*(1-Elteq!$F$9)","v":2.9318874303676736},"8591735025052"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"KS 11",null,"Kabelová spona přírodní plastová pro svazek o průměru 10-13mm","100ks",4.4906123933479556,{"$f":"F2374*(1-Elteq!$F$9)","v":4.4906123933479556},"8591735025069"]
["TECHNIK","KS 15",null,"Kabelová spona přírodní plastová pro svazek o průměru 13-16mm","100ks",5.3070873739566746,{"$f":"F2375*(1-Elteq!$F$9)","v":5.3070873739566746},"8591735025076"]
["TECHNIK","KS 18",null,"Kabelová spona přírodní plastová pro svazek o průměru 16-20mm","100ks",6.1235623545653937,{"$f":"F2376*(1-Elteq!$F$9)","v":6.1235623545653937},"8591735025083"]
["TECHNIK","KS 24",null,"Kabelová spona přírodní plastová pro svazek o průměru 20-26mm","100ks",7.236937328122738,{"$f":"F2377*(1-Elteq!$F$9)","v":7.236937328122738},"8591735025090"]
["TECHNIK","KSU 12",null,"Kabelová svorka přírodní samolepicí pro průměr 9,0-12,0mm","100ks",17.81399957691751,{"$f":"F2378*(1-Elteq!$F$9)","v":17.81399957691751},"8591735056650"]
["TECHNIK","KSU 12 G",null,"Kabelová svorka přírodní samolepicí pro průměr 9,0-12,0mm","100ks",8.8327747902215989,{"$f":"F2379*(1-Elteq!$F$9)","v":8.8327747902215989},"8591735034726"]
["TECHNIK","KSU 14",null,"Kabelová svorka přírodní samolepicí pro průměr 11,9-14,3mm","100ks",20.782999506403762,{"$f":"F2380*(1-Elteq!$F$9)","v":20.782999506403762},"8591735034733"]
["TECHNIK","KSU 19",null,"Kabelová svorka přírodní samolepicí pro průměr 14,7-19,1mm","100ks",32.25076173404441,{"$f":"F2381*(1-Elteq!$F$9)","v":32.25076173404441},"8591735034740"]
["TECHNIK","KSU 23",null,"Kabelová svorka přírodní samolepicí pro průměr 22,2-25,4mm","100ks",28.205499330119391,{"$f":"F2382*(1-Elteq!$F$9)","v":28.205499330119391},"8591735034757"]
["TECHNIK","KSUC  6",null,"Kabelová svorka černá samolepicí pro průměr 6mm","100ks",18.370687063696181,{"$f":"F2383*(1-Elteq!$F$9)","v":18.370687063696181},"8591735034764"]
["TECHNIK","KSUC  9",null,"Kabelová svorka černá samolepicí pro průměr 9mm","100ks",19.298499541660636,{"$f":"F2384*(1-Elteq!$F$9)","v":19.298499541660636},"8591735034771"]
["TECHNIK","KSUC 12",null,"Kabelová svorka černá samolepicí pro průměr 12mm","100ks",15.216124638617039,{"$f":"F2385*(1-Elteq!$F$9)","v":15.216124638617039},"8591735034788"]
["TECHNIK","KSUC 14",null,"Kabelová svorka černá samolepicí pro průměr 14mm","100ks",18.370687063696181,{"$f":"F2386*(1-Elteq!$F$9)","v":18.370687063696181},"8591735034795"]
["TECHNIK","KSUC 16",null,"Kabelová svorka černá samolepicí pro průměr 16mm","100ks",18.927374550474855,{"$f":"F2387*(1-Elteq!$F$9)","v":18.927374550474855},"8591735034863"]
["TECHNIK","KSUC 18",null,"Kabelová svorka černá samolepicí pro průměr 18mm","100ks",19.855187028439307,{"$f":"F2388*(1-Elteq!$F$9)","v":19.855187028439307},"8591735034856"]
["TECHNIK","KSUS  7",null,"Kabelová svorka šedá samolepicí pro průměr 6-7mm","100ks",20.263424518743669,{"$f":"F2389*(1-Elteq!$F$9)","v":20.263424518743669},"8591735034849"]
["TECHNIK","KSUS  8",null,"Kabelová svorka šedá samolepicí pro průměr 7-8mm","100ks",29.801336792218251,{"$f":"F2390*(1-Elteq!$F$9)","v":29.801336792218251},"8591735034832"]
["TECHNIK","KSUS 10",null,"Kabelová svorka šedá samolepicí pro průměr 9-10mm","100ks",34.700186675870569,{"$f":"F2391*(1-Elteq!$F$9)","v":34.700186675870569},"8591735034825"]
["TECHNIK","KSUS 14",null,"Kabelová svorka šedá samolepicí pro průměr 12-14mm","100ks",36.555811631799472,{"$f":"F2392*(1-Elteq!$F$9)","v":36.555811631799472},"8591735034818"]
["TECHNIK","KSUS 18",null,"Kabelová svorka šedá samolepicí pro průměr 16-18mm","100ks",43.050498977550646,{"$f":"F2393*(1-Elteq!$F$9)","v":43.050498977550646},"8591735034801"]
["TECHNIK","OTR  7",null,"Ochranná trubice s podélným prořezem, vnitřní průměr   7,4mm Polypropylen, stálost -40°C až +80°C","300m",109.85299739099131,{"$f":"F2394*(1-Elteq!$F$9)","v":109.85299739099131},"8591735051891"]
["TECHNIK","OTR 11",null,"Ochranná trubice s podélným prořezem, vnitřní průměr 10,7mm Polypropylen, stálost -40°C až +80°C","200m",84.61649799035817,{"$f":"F2395*(1-Elteq!$F$9)","v":84.61649799035817},"8591735051907"]
["TECHNIK","OTR 13",null,"Ochranná trubice s podélným prořezem, vnitřní průměr 13,2mm Polypropylen, stálost -40°C až +80°C","200m",104.2861225232046,{"$f":"F2396*(1-Elteq!$F$9)","v":104.2861225232046},"8591735051914"]
["TECHNIK","OTR 15",null,"Ochranná trubice s podélným prořezem, vnitřní průměr 15,0mm Polypropylen, stálost -40°C až +80°C","100m",56.039873669053001,{"$f":"F2397*(1-Elteq!$F$9)","v":56.039873669053001},"8591735051921"]
["TECHNIK","OTR 19",null,"Ochranná trubice s podélným prořezem, vnitřní průměr 19,3mm Polypropylen, stálost -40°C až +80°C","100m",70.88487331648426,{"$f":"F2398*(1-Elteq!$F$9)","v":70.88487331648426},"8591735051938"]
["TECHNIK","OTR 22",null,"Ochranná trubice s podélným prořezem, vnitřní průměr 22,2mm Polypropylen, stálost -40°C až +80°C","100m",74.224998237156285,{"$f":"F2399*(1-Elteq!$F$9)","v":74.224998237156285},"8591735051945"]
["TECHNIK","OTR 25",null,"Ochranná trubice s podélným prořezem, vnitřní průměr 25,0mm Polypropylen, stálost -40°C až +80°C","50m",46.019498907036898,{"$f":"F2400*(1-Elteq!$F$9)","v":46.019498907036898},"8591735051952"]
["TECHNIK","OTR 28",null,"Ochranná trubice s podélným prořezem, vnitřní průměr 28,2mm Polypropylen, stálost -40°C až +80°C","50m",54.184248713124092,{"$f":"F2401*(1-Elteq!$F$9)","v":54.184248713124092},"8591735051969"]
["TECHNIK","OTR 32",null,"Ochranná trubice s podélným prořezem, vnitřní průměr 32,4mm Polypropylen, stálost -40°C až +80°C","50m",80.534123087314583,{"$f":"F2402*(1-Elteq!$F$9)","v":80.534123087314583},"8591735053314"]
["TECHNIK","PE-HB-05 černá",null,"Ochranný oplet pro průměr   4 - 9mm CANUFLEX Polyester, stálost -50°C až +150°C, krátkodobě +200°C","500m",113.41579730637481,{"$f":"F2403*(1-Elteq!$F$9)","v":113.41579730637481},"8591735052232"]
["TECHNIK","PE-HB-10 černá",null,"Ochranný oplet pro průměr   9-15mm CANUFLEX Polyester, stálost -50°C až +150°C, krátkodobě +200°C","300m",113.00755981607045,{"$f":"F2404*(1-Elteq!$F$9)","v":113.00755981607045},"8591735052249"]
["TECHNIK","PE-HB-15 černá",null,"Ochranný oplet pro průměr 10-20mm CANUFLEX Polyester, stálost -50°C až +150°C, krátkodobě +200°C","300m",215.88340737276908,{"$f":"F2405*(1-Elteq!$F$9)","v":215.88340737276908},"8591735052256"]
["TECHNIK","PE-HB-20 černá",null,"Ochranný oplet pro průměr 15-26mm CANUFLEX Polyester, stálost -50°C až +150°C, krátkodobě +200°C","200m",160.17754619578326,{"$f":"F2406*(1-Elteq!$F$9)","v":160.17754619578326},"8591735052263"]
["TECHNIK","PE-HB-50 černá",null,"Ochranný oplet pro průměr 40-60mm CANUFLEX Polyester, stálost -50°C až +150°C, krátkodobě +200°C","50m",115.75388475084523,{"$f":"F2407*(1-Elteq!$F$9)","v":115.75388475084523},"8591735056452"]
["TECHNIK","VP 2,5x100 fialová",null,"Vázací páska do 8kg, rozměr 2,5x100mm, barva fialová","100ks",0.59379998589725036,{"$f":"F2408*(1-Elteq!$F$9)","v":0.59379998589725036},"8591735049317"]
["TECHNIK","VP 2,5x100 hnědá",null,"Vázací páska do 8kg, rozměr 2,5x100mm, barva hnědá","100ks",0.59379998589725036,{"$f":"F2409*(1-Elteq!$F$9)","v":0.59379998589725036},"8591735034313"]
["TECHNIK","VP 2,5x100 modrá",null,"Vázací páska do 8kg, rozměr 2,5x100mm, barva modrá","100ks",0.59379998589725036,{"$f":"F2410*(1-Elteq!$F$9)","v":0.59379998589725036},"8591735021955"]
["TECHNIK","VP 2,5x100 oranžová",null,"Vázací páska do 8kg, rozměr 2,5x100mm, barva oranžová","100ks",0.59379998589725036,{"$f":"F2411*(1-Elteq!$F$9)","v":0.59379998589725036},"8591735034320"]
["TECHNIK","VP 2,5x100 rudá",null,"Vázací páska do 8kg, rozměr 2,5x100mm, barva rudá","100ks",0.59379998589725036,{"$f":"F2412*(1-Elteq!$F$9)","v":0.59379998589725036},"8591735021962"]
["TECHNIK","VP 2,5x100 šedá",null,"Vázací páska do 8kg, rozměr 2,5x100mm, barva šedá","100ks",0.59379998589725036,{"$f":"F2413*(1-Elteq!$F$9)","v":0.59379998589725036},"8591735049324"]
["TECHNIK","VP 2,5x100 zelená",null,"Vázací páska do 8kg, rozměr 2,5x100mm, barva zelená","100ks",0.59379998589725036,{"$f":"F2414*(1-Elteq!$F$9)","v":0.59379998589725036},"8591735021979"]
["TECHNIK","VP 2,5x100 žlutá",null,"Vázací páska do 8kg, rozměr 2,5x100mm, barva žlutá","100ks",0.59379998589725036,{"$f":"F2415*(1-Elteq!$F$9)","v":0.59379998589725036},"8591735021986"]
["TECHNIK","VP 2,5x200 fialová",null,"Vázací páska do 8kg, rozměr 2,5x200mm, barva fialová","100ks",1.4844999647431258,{"$f":"F2416*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735011031"]
["TECHNIK","VP 2,5x200 hnědá",null,"Vázací páska do 8kg, rozměr 2,5x200mm, barva hnědá","100ks",1.4844999647431258,{"$f":"F2417*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735011451"]
["TECHNIK","VP 2,5x200 modrá",null,"Vázací páska do 8kg, rozměr 2,5x200mm, barva modrá","100ks",1.4844999647431258,{"$f":"F2418*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735021993"]
["TECHNIK","VP 2,5x200 oranžová",null,"Vázací páska do 8kg, rozměr 2,5x200mm, barva oranžová","100ks",1.4844999647431258,{"$f":"F2419*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735032142"]
["TECHNIK","VP 2,5x200 rudá",null,"Vázací páska do 8kg, rozměr 2,5x200mm, barva rudá","100ks",1.4844999647431258,{"$f":"F2420*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735022006"]
["TECHNIK","VP 2,5x200 šedá",null,"Vázací páska do 8kg, rozměr 2,5x200mm, barva šedá","100ks",1.4844999647431258,{"$f":"F2421*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735032159"]
["TECHNIK","VP 2,5x200 zelená",null,"Vázací páska do 8kg, rozměr 2,5x200mm, barva zelená","100ks",1.4844999647431258,{"$f":"F2422*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735022013"]
["TECHNIK","VP 2,5x200 žlutá",null,"Vázací páska do 8kg, rozměr 2,5x200mm, barva žlutá","100ks",1.4844999647431258,{"$f":"F2423*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735022020"]
["TECHNIK","VP 3,6x140 hnědá",null,"Vázací páska do 18kg, rozměr 3,6x140mm, barva hnědá","100ks",1.781399957691751,{"$f":"F2424*(1-Elteq!$F$9)","v":1.781399957691751},"8591735032166"]
["TECHNIK","VP 3,6x140 modrá",null,"Vázací páska do 18kg, rozměr 3,6x140mm, barva modrá","100ks",1.781399957691751,{"$f":"F2425*(1-Elteq!$F$9)","v":1.781399957691751},"8591735022037"]
["TECHNIK","VP 3,6x140 oranžová",null,"Vázací páska do 18kg, rozměr 3,6x140mm, barva oranžová","100ks",1.781399957691751,{"$f":"F2426*(1-Elteq!$F$9)","v":1.781399957691751},"8591735049331"]
["TECHNIK","VP 3,6x140 rudá",null,"Vázací páska do 18kg, rozměr 3,6x140mm, barva rudá","100ks",1.781399957691751,{"$f":"F2427*(1-Elteq!$F$9)","v":1.781399957691751},"8591735022044"]
["TECHNIK","VP 3,6x140 šedá",null,"Vázací páska do 18kg, rozměr 3,6x140mm, barva šedá","100ks",1.781399957691751,{"$f":"F2428*(1-Elteq!$F$9)","v":1.781399957691751},"8591735032173"]
["TECHNIK","VP 3,6x140 zelená",null,"Vázací páska do 18kg, rozměr 3,6x140mm, barva zelená","100ks",1.781399957691751,{"$f":"F2429*(1-Elteq!$F$9)","v":1.781399957691751},"8591735022051"]
["TECHNIK","VP 3,6x140 zelená UV",null,"Vázací páska do 18kg, rozměr 3,6x140mm, dlouhodobě UV stabilní, barva zelená","100ks",2.041187451521798,{"$f":"F2430*(1-Elteq!$F$9)","v":2.041187451521798},"8591735056018"]
["TECHNIK","VP 3,6x140 žlutá",null,"Vázací páska do 18kg, rozměr 3,6x140mm, barva žlutá","100ks",1.781399957691751,{"$f":"F2431*(1-Elteq!$F$9)","v":1.781399957691751},"8591735022068"]
["TECHNIK","VP 3,6x200 fialová",null,"Vázací páska do 18kg, rozměr 3,6x200mm, barva fialová","100ks",2.3751999435890014,{"$f":"F2432*(1-Elteq!$F$9)","v":2.3751999435890014},"8591735043919"]
["TECHNIK","VP 3,6x200 modrá",null,"Vázací páska do 18kg, rozměr 3,6x200mm, barva modrá","100ks",2.3751999435890014,{"$f":"F2433*(1-Elteq!$F$9)","v":2.3751999435890014},"8591735022075"]
["TECHNIK","VP 3,6x200 oranžová",null,"Vázací páska do 18kg, rozměr 3,6x200mm, barva oranžová","100ks",2.3751999435890014,{"$f":"F2434*(1-Elteq!$F$9)","v":2.3751999435890014},"8591735049980"]
["TECHNIK","VP 3,6x200 rudá",null,"Vázací páska do 18kg, rozměr 3,6x200mm, barva rudá","100ks",2.3751999435890014,{"$f":"F2435*(1-Elteq!$F$9)","v":2.3751999435890014},"8591735022082"]
["TECHNIK","VP 3,6x200 šedá",null,"Vázací páska do 18kg, rozměr 3,6x200mm, barva šedá","100ks",2.3751999435890014,{"$f":"F2436*(1-Elteq!$F$9)","v":2.3751999435890014},"8591735043926"]
["TECHNIK","VP 3,6x200 zelená",null,"Vázací páska do 18kg, rozměr 3,6x200mm, barva zelená","100ks",2.3751999435890014,{"$f":"F2437*(1-Elteq!$F$9)","v":2.3751999435890014},"8591735022099"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"VP 3,6x200 žlutá",null,"Vázací páska do 18kg, rozměr 3,6x200mm, barva žlutá","100ks",2.3751999435890014,{"$f":"F2438*(1-Elteq!$F$9)","v":2.3751999435890014},"8591735022105"]
["TECHNIK","VP 3,6x300 modrá",null,"Vázací páska do 18kg, rozměr 3,6x292mm, barva modrá","100ks",3.59991241450208,{"$f":"F2439*(1-Elteq!$F$9)","v":3.59991241450208},"8591735022112"]
["TECHNIK","VP 3,6x300 rudá",null,"Vázací páska do 18kg, rozměr 3,6x292mm, barva rudá","100ks",3.59991241450208,{"$f":"F2440*(1-Elteq!$F$9)","v":3.59991241450208},"8591735022129"]
["TECHNIK","VP 3,6x300 zelená",null,"Vázací páska do 18kg, rozměr 3,6x292mm, barva zelená","100ks",3.59991241450208,{"$f":"F2441*(1-Elteq!$F$9)","v":3.59991241450208},"8591735022136"]
["TECHNIK","VP 3,6x300 žlutá",null,"Vázací páska do 18kg, rozměr 3,6x292mm, barva žlutá","100ks",3.59991241450208,{"$f":"F2442*(1-Elteq!$F$9)","v":3.59991241450208},"8591735022143"]
["TECHNIK","VP 4,8x200 fialová",null,"Vázací páska do 22kg, rozměr 4,8x200mm, barva fialová","100ks",2.8576624321305171,{"$f":"F2443*(1-Elteq!$F$9)","v":2.8576624321305171},"8591735049379"]
["TECHNIK","VP 4,8x200 hnědá",null,"Vázací páska do 22kg, rozměr 4,8x200mm, barva hnědá","100ks",2.8576624321305171,{"$f":"F2444*(1-Elteq!$F$9)","v":2.8576624321305171},"8591735049348"]
["TECHNIK","VP 4,8x200 modrá",null,"Vázací páska do 22kg, rozměr 4,8x200mm, barva modrá","100ks",2.8576624321305171,{"$f":"F2445*(1-Elteq!$F$9)","v":2.8576624321305171},"8591735022150"]
["TECHNIK","VP 4,8x200 oranžová",null,"Vázací páska do 22kg, rozměr 4,8x200mm, barva oranžová","100ks",2.8576624321305171,{"$f":"F2446*(1-Elteq!$F$9)","v":2.8576624321305171},"8591735049355"]
["TECHNIK","VP 4,8x200 rudá",null,"Vázací páska do 22kg, rozměr 4,8x200mm, barva rudá","100ks",2.8576624321305171,{"$f":"F2447*(1-Elteq!$F$9)","v":2.8576624321305171},"8591735022167"]
["TECHNIK","VP 4,8x200 šedá",null,"Vázací páska do 22kg, rozměr 4,8x200mm, barva šedá","100ks",2.8576624321305171,{"$f":"F2448*(1-Elteq!$F$9)","v":2.8576624321305171},"8591735049362"]
["TECHNIK","VP 4,8x200 zelená",null,"Vázací páska do 22kg, rozměr 4,8x200mm, barva zelená","100ks",2.8576624321305171,{"$f":"F2449*(1-Elteq!$F$9)","v":2.8576624321305171},"8591735022174"]
["TECHNIK","VP 4,8x200 zelená UV",null,"Vázací páska do 22kg, rozměr 4,8x200mm, dlouhodobě UV stabilní, barva zelená","100ks",3.265899922434877,{"$f":"F2450*(1-Elteq!$F$9)","v":3.265899922434877},"8591735055998"]
["TECHNIK","VP 4,8x200 žlutá",null,"Vázací páska do 22kg, rozměr 4,8x200mm, barva žlutá","100ks",2.8576624321305171,{"$f":"F2451*(1-Elteq!$F$9)","v":2.8576624321305171},"8591735022181"]
["TECHNIK","VP 4,8x250 fialová",null,"Vázací páska do 22kg, rozměr 4,8x250mm, barva fialová","100ks",3.6370249136206585,{"$f":"F2452*(1-Elteq!$F$9)","v":3.6370249136206585},"8591735042356"]
["TECHNIK","VP 4,8x250 modrá",null,"Vázací páska do 22kg, rozměr 4,8x250mm, barva modrá","100ks",3.6370249136206585,{"$f":"F2453*(1-Elteq!$F$9)","v":3.6370249136206585},"8591735022198"]
["TECHNIK","VP 4,8x250 rudá",null,"Vázací páska do 22kg, rozměr 4,8x250mm, barva rudá","100ks",3.6370249136206585,{"$f":"F2454*(1-Elteq!$F$9)","v":3.6370249136206585},"8591735022204"]
["TECHNIK","VP 4,8x250 šedá",null,"Vázací páska do 22kg, rozměr 4,8x250mm, barva šedá","100ks",3.6370249136206585,{"$f":"F2455*(1-Elteq!$F$9)","v":3.6370249136206585},"8591735042363"]
["TECHNIK","VP 4,8x250 zelená",null,"Vázací páska do 22kg, rozměr 4,8x250mm, barva zelená","100ks",3.6370249136206585,{"$f":"F2456*(1-Elteq!$F$9)","v":3.6370249136206585},"8591735022211"]
["TECHNIK","VP 4,8x250 žlutá",null,"Vázací páska do 22kg, rozměr 4,8x250mm, barva žlutá","100ks",3.6370249136206585,{"$f":"F2457*(1-Elteq!$F$9)","v":3.6370249136206585},"8591735022228"]
["TECHNIK","VP 4,8x300 fialová",null,"Vázací páska do 22kg, rozměr 4,8x300mm, barva fialová","100ks",4.2679373986364864,{"$f":"F2458*(1-Elteq!$F$9)","v":4.2679373986364864},"8591735047313"]
["TECHNIK","VP 4,8x300 hnědá",null,"Vázací páska do 22kg, rozměr 4,8x300mm, barva hnědá","100ks",4.2679373986364864,{"$f":"F2459*(1-Elteq!$F$9)","v":4.2679373986364864},"8591735047283"]
["TECHNIK","VP 4,8x300 modrá",null,"Vázací páska do 22kg, rozměr 4,8x300mm, barva modrá","100ks",4.2679373986364864,{"$f":"F2460*(1-Elteq!$F$9)","v":4.2679373986364864},"8591735022235"]
["TECHNIK","VP 4,8x300 oranžová",null,"Vázací páska do 22kg, rozměr 4,8x300mm, barva oranžová","100ks",4.2679373986364864,{"$f":"F2461*(1-Elteq!$F$9)","v":4.2679373986364864},"8591735047306"]
["TECHNIK","VP 4,8x300 rudá",null,"Vázací páska do 22kg, rozměr 4,8x300mm, barva rudá","100ks",4.2679373986364864,{"$f":"F2462*(1-Elteq!$F$9)","v":4.2679373986364864},"8591735022242"]
["TECHNIK","VP 4,8x300 šedá",null,"Vázací páska do 22kg, rozměr 4,8x300mm, barva šedá","100ks",4.2679373986364864,{"$f":"F2463*(1-Elteq!$F$9)","v":4.2679373986364864},"8591735047290"]
["TECHNIK","VP 4,8x300 zelená",null,"Vázací páska do 22kg, rozměr 4,8x300mm, barva zelená","100ks",4.2679373986364864,{"$f":"F2464*(1-Elteq!$F$9)","v":4.2679373986364864},"8591735022259"]
["TECHNIK","VP 4,8x300 žlutá",null,"Vázací páska do 22kg, rozměr 4,8x300mm, barva žlutá","100ks",4.2679373986364864,{"$f":"F2465*(1-Elteq!$F$9)","v":4.2679373986364864},"8591735022266"]
["TECHNIK","VP 4,8x370 hnědá",null,"Vázací páska do 22kg, rozměr 4,8x368mm, barva hnědá","100ks",5.3813123721938307,{"$f":"F2466*(1-Elteq!$F$9)","v":5.3813123721938307},"8591735054007"]
["TECHNIK","VP 4,8x370 modrá",null,"Vázací páska do 22kg, rozměr 4,8x368mm, barva modrá","100ks",5.3813123721938307,{"$f":"F2467*(1-Elteq!$F$9)","v":5.3813123721938307},"8591735022273"]
["TECHNIK","VP 4,8x370 rudá",null,"Vázací páska do 22kg, rozměr 4,8x368mm, barva rudá","100ks",5.3813123721938307,{"$f":"F2468*(1-Elteq!$F$9)","v":5.3813123721938307},"8591735022280"]
["TECHNIK","VP 4,8x370 zelená",null,"Vázací páska do 22kg, rozměr 4,8x368mm, barva zelená","100ks",5.3813123721938307,{"$f":"F2469*(1-Elteq!$F$9)","v":5.3813123721938307},"8591735022297"]
["TECHNIK","VP 4,8x370 žlutá",null,"Vázací páska do 22kg, rozměr 4,8x368mm, barva žlutá","100ks",5.3813123721938307,{"$f":"F2470*(1-Elteq!$F$9)","v":5.3813123721938307},"8591735022303"]
["TECHNIK","VP 7,6x250 zelená UV",null,"Vázací páska do 54kg, rozměr 7,6x250mm, dlouhodobě UV stabilní, barva zelená","100ks",9.8348122664232083,{"$f":"F2471*(1-Elteq!$F$9)","v":9.8348122664232083},"8591735056001"]
["TECHNIK","VP 7,6x370 modrá",null,"Vázací páska do 54kg, rozměr 7,6x370mm, barva modrá","100ks",11.356424730284912,{"$f":"F2472*(1-Elteq!$F$9)","v":11.356424730284912},"8591735056377"]
["TECHNIK","VP 7,6x370 rudá",null,"Vázací páska do 54kg, rozměr 7,6x370mm, barva rudá","100ks",11.356424730284912,{"$f":"F2473*(1-Elteq!$F$9)","v":11.356424730284912},"8591735036799"]
["TECHNIK","VP 7,6x370 zelená",null,"Vázací páska do 54kg, rozměr 7,6x370mm, barva zelená","100ks",11.356424730284912,{"$f":"F2474*(1-Elteq!$F$9)","v":11.356424730284912},"8591735056261"]
["TECHNIK","VP 7,6x370 žlutá",null,"Vázací páska do 54kg, rozměr 7,6x370mm, barva žlutá","100ks",11.356424730284912,{"$f":"F2475*(1-Elteq!$F$9)","v":11.356424730284912},"8591735056278"]
["TECHNIK","VP 9,0x530 zelená",null,"Vázací páska do 54kg, rozměr 9,0x530mm, barva zelená","100ks",16.663512104241587,{"$f":"F2476*(1-Elteq!$F$9)","v":16.663512104241587},""]
["TECHNIK","VP 9,0x780 šedá",null,"Vázací páska do 54kg, rozměr 9,0x780mm, barva šedá","100ks",25.756074388293232,{"$f":"F2477*(1-Elteq!$F$9)","v":25.756074388293232},""]
["TECHNIK","VPC  1,7x70",null,"Vázací páska černá krátkodobě UV odolná, nosnost 3kg, průměr svazku 11mm, rozměr 1,7x70mm","100ks",0.70513748325298475,{"$f":"F2478*(1-Elteq!$F$9)","v":0.70513748325298475},"8591735051822"]
["TECHNIK","VPC  1,9x100",null,"Vázací páska černá krátkodobě UV odolná, nosnost 5kg, průměr svazku 22mm, rozměr 1,95x103mm","100ks",0.81647498060871926,{"$f":"F2479*(1-Elteq!$F$9)","v":0.81647498060871926},"8591735051839"]
["TECHNIK","VPC  2,4x60",null,"Vázací páska černá krátkodobě UV odolná, nosnost 8kg, průměr svazku 11mm, rozměr 2,4x60mm","100ks",0.42679373986364866,{"$f":"F2480*(1-Elteq!$F$9)","v":0.42679373986364866},"8591735022846"]
["TECHNIK","VPC  2,4x80",null,"Vázací páska černá krátkodobě UV odolná, nosnost 8kg, průměr svazku 15mm, rozměr 2,4x80mm","100ks",0.46390623898222683,{"$f":"F2481*(1-Elteq!$F$9)","v":0.46390623898222683},"8591735004965"]
["TECHNIK","VPC  2,5x100",null,"Vázací páska černá krátkodobě UV odolná, nosnost 8kg, průměr svazku 22mm, rozměr 2,5x100mm","100ks",0.37112499118578146,{"$f":"F2482*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735004972"]
["TECHNIK","VPC  2,5x100 UV",null,"Vázací páska černá dlouhodobě UV stabilní, nosnost 8kg, průměr svazku 22mm, rozměr 2,5x100mm","100ks",0.48246248854151591,{"$f":"F2483*(1-Elteq!$F$9)","v":0.48246248854151591},"8591735050702"]
["TECHNIK","VPC  2,5x100/1000",null,"Vázací páska černá krátkodobě UV odolná, nosnost 8kg, průměr svazku 22mm, rozměr 2,5x100mm (1000ks)","1000ks",3.7112499118578146,{"$f":"F2484*(1-Elteq!$F$9)","v":3.7112499118578146},"8591735037871"]
["TECHNIK","VPC  2,5x120",null,"Vázací páska černá krátkodobě UV odolná, nosnost 8kg, průměr svazku 30mm, rozměr 2,5x120mm","100ks",0.59379998589725036,{"$f":"F2485*(1-Elteq!$F$9)","v":0.59379998589725036},"8591735008383"]
["TECHNIK","VPC  2,5x140",null,"Vázací páska černá krátkodobě UV odolná, nosnost 8kg, průměr svazku 33mm, rozměr 2,5x140mm","100ks",0.64946873457511756,{"$f":"F2486*(1-Elteq!$F$9)","v":0.64946873457511756},"8591735004996"]
["TECHNIK","VPC  2,5x160",null,"Vázací páska černá krátkodobě UV odolná, nosnost 8kg, průměr svazku 40mm, rozměr 2,5x160mm","100ks",0.77936248149014109,{"$f":"F2487*(1-Elteq!$F$9)","v":0.77936248149014109},"8591735005009"]
["TECHNIK","VPC  2,5x200",null,"Vázací páska černá krátkodobě UV odolná, nosnost 8kg, průměr svazku 53mm, rozměr 2,5x200mm","100ks",0.83503123016800829,{"$f":"F2488*(1-Elteq!$F$9)","v":0.83503123016800829},"8591735005016"]
["TECHNIK","VPC  2,5x200/1000",null,"Vázací páska černá krátkodobě UV odolná, nosnost 8kg, průměr svazku 53mm, rozměr 2,5x200mm (1000ks)","1000ks",8.3503123016800824,{"$f":"F2489*(1-Elteq!$F$9)","v":8.3503123016800824},"8591735048488"]
["TECHNIK","VPC  3,6x140",null,"Vázací páska černá krátkodobě UV odolná, nosnost 18kg, průměr svazku 33mm, rozměr 3,6x140mm","100ks",0.70513748325298475,{"$f":"F2490*(1-Elteq!$F$9)","v":0.70513748325298475},"8591735005023"]
["TECHNIK","VPC  3,6x140 UV",null,"Vázací páska černá dlouhodobě UV stabilní, nosnost 18kg, průměr svazku 33mm, rozměr 3,6x140mm","100ks",1.0577062248794771,{"$f":"F2491*(1-Elteq!$F$9)","v":1.0577062248794771},"8591735050719"]
["TECHNIK","VPC  3,6x140/1000",null,"Vázací páska černá krátkodobě UV odolná, nosnost 18kg, průměr svazku 33mm, rozměr 3,6x140mm (1000ks)","1000ks",7.0513748325298478,{"$f":"F2492*(1-Elteq!$F$9)","v":7.0513748325298478},"8591735041946"]
["TECHNIK","VPC  3,6x150",null,"Vázací páska černá krátkodobě UV odolná, nosnost 18kg, průměr svazku 35mm, rozměr 3,6x150mm","100ks",1.0577062248794771,{"$f":"F2493*(1-Elteq!$F$9)","v":1.0577062248794771},"8591735011130"]
["TECHNIK","VPC  3,6x180",null,"Vázací páska černá krátkodobě UV odolná, nosnost 18kg, průměr svazku 47mm, rozměr 3,6x180mm","100ks",1.4288312160652585,{"$f":"F2494*(1-Elteq!$F$9)","v":1.4288312160652585},"8591735020910"]
["TECHNIK","VPC  3,6x200",null,"Vázací páska černá krátkodobě UV odolná, nosnost 18kg, průměr svazku 53mm, rozměr 3,6x200mm","100ks",1.4473874656245478,{"$f":"F2495*(1-Elteq!$F$9)","v":1.4473874656245478},"8591735005030"]
["TECHNIK","VPC  3,6x200 UV",null,"Vázací páska černá dlouhodobě UV stabilní, nosnost 18kg, průměr svazku 53mm, rozměr 3,6x200mm","100ks",1.7628437081324619,{"$f":"F2496*(1-Elteq!$F$9)","v":1.7628437081324619},"8591735050726"]
["TECHNIK","VPC  3,6x250",null,"Vázací páska černá krátkodobě UV odolná, nosnost 18kg, průměr svazku 65mm, rozměr 3,6x250mm","100ks",1.8185124568103292,{"$f":"F2497*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735019136"]
["TECHNIK","VPC  3,6x300",null,"Vázací páska černá krátkodobě UV odolná, nosnost 18kg, průměr svazku 76mm, rozměr 3,6x292mm","100ks",1.8370687063696183,{"$f":"F2498*(1-Elteq!$F$9)","v":1.8370687063696183},"8591735005047"]
["TECHNIK","VPC  3,6x370",null,"Vázací páska černá krátkodobě UV odolná, nosnost 18kg, průměr svazku 102mm, rozměr 3,6x370mm","100ks",2.6535436869783373,{"$f":"F2499*(1-Elteq!$F$9)","v":2.6535436869783373},"8591735005054"]
["TECHNIK","VPC  4,8x120",null,"Vázací páska černá krátkodobě UV odolná, nosnost 22kg, průměr svazku 28mm, rozměr 4,8x120mm","100ks",1.4102749665059695,{"$f":"F2500*(1-Elteq!$F$9)","v":1.4102749665059695},"8591735022853"]
["TECHNIK","VPC  4,8x160",null,"Vázací páska černá krátkodobě UV odolná, nosnost 22kg, průměr svazku 38mm, rozměr 4,8x160mm","100ks",1.4473874656245478,{"$f":"F2501*(1-Elteq!$F$9)","v":1.4473874656245478},"8591735010652"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"VPC  4,8x188",null,"Vázací páska černá krátkodobě UV odolná, nosnost 22kg, průměr svazku 46mm, rozměr 4,8x188mm","100ks",1.4659437151838368,{"$f":"F2502*(1-Elteq!$F$9)","v":1.4659437151838368},"8591735010638"]
["TECHNIK","VPC  4,8x200",null,"Vázací páska černá krátkodobě UV odolná, nosnost 22kg, průměr svazku 50mm, rozměr 4,8x200mm","100ks",1.4844999647431258,{"$f":"F2503*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735005078"]
["TECHNIK","VPC  4,8x200 UV",null,"Vázací páska černá dlouhodobě UV stabilní, nosnost 22kg, průměr svazku 50mm, rozměr 4,8x200mm","100ks",1.8185124568103292,{"$f":"F2504*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735050733"]
["TECHNIK","VPC  4,8x200 Z",null,"Vázací páska černá UV se zoubky na vnější straně pro ochranu kabelů, nosnost 22kg, prům. svazku 50mm","500ks",8.1647498060871921,{"$f":"F2505*(1-Elteq!$F$9)","v":8.1647498060871921},"8591735053598"]
["TECHNIK","VPC  4,8x200/1000",null,"Vázací páska černá krátkodobě UV odolná, nosnost 22kg, průměr svazku 50mm, rozměr 4,8x200mm (1000ks)","1000ks",14.844999647431258,{"$f":"F2506*(1-Elteq!$F$9)","v":14.844999647431258},"8591735041953"]
["TECHNIK","VPC  4,8x250",null,"Vázací páska černá krátkodobě UV odolná, nosnost 22kg, průměr svazku 60mm, rozměr 4,8x250mm","100ks",2.1525249488775327,{"$f":"F2507*(1-Elteq!$F$9)","v":2.1525249488775327},"8591735005085"]
["TECHNIK","VPC  4,8x280",null,"Vázací páska černá krátkodobě UV odolná, nosnost 22kg, průměr svazku 70mm, rozměr 4,8x280mm","100ks",2.2453061966739778,{"$f":"F2508*(1-Elteq!$F$9)","v":2.2453061966739778},"8591735005092"]
["TECHNIK","VPC  4,8x300",null,"Vázací páska černá krátkodobě UV odolná, nosnost 22kg, průměr svazku 76mm, rozměr 4,8x300mm","100ks",2.2824186957925559,{"$f":"F2509*(1-Elteq!$F$9)","v":2.2824186957925559},"8591735004989"]
["TECHNIK","VPC  4,8x300 UV",null,"Vázací páska černá dlouhodobě UV stabilní, nosnost 22kg, průměr svazku 76mm, rozměr 4,8x300mm","100ks",2.783437433893361,{"$f":"F2510*(1-Elteq!$F$9)","v":2.783437433893361},"8591735050740"]
["TECHNIK","VPC  4,8x300/1000",null,"Vázací páska černá krátkodobě UV odolná, nosnost 22kg, průměr svazku 76mm, rozměr 4,8x300mm (1000ks)","1000ks",22.824186957925559,{"$f":"F2511*(1-Elteq!$F$9)","v":22.824186957925559},"8591735048495"]
["TECHNIK","VPC  4,8x370",null,"Vázací páska černá krátkodobě UV odolná, nosnost 22kg, průměr svazku 102mm, rozměr 4,8x368mm","100ks",2.5422061896226031,{"$f":"F2512*(1-Elteq!$F$9)","v":2.5422061896226031},"8591735005108"]
["TECHNIK","VPC  4,8x385",null,"Vázací páska černá krátkodobě UV odolná, nosnost 22kg, průměr svazku 106mm, rozměr 4,8x385mm","100ks",3.8225874092135492,{"$f":"F2513*(1-Elteq!$F$9)","v":3.8225874092135492},"8591735042066"]
["TECHNIK","VPC  4,8x430",null,"Vázací páska černá krátkodobě UV odolná, nosnost 22kg, průměr svazku 110mm, rozměr 4,8x430mm","100ks",4.9359623827708932,{"$f":"F2514*(1-Elteq!$F$9)","v":4.9359623827708932},"8591735005122"]
["TECHNIK","VPC  4,8x530",null,"Vázací páska černá krátkodobě UV odolná, nosnost 22kg, průměr svazku 140mm, rozměr 4,8x530mm","100ks",7.7565123157828326,{"$f":"F2515*(1-Elteq!$F$9)","v":7.7565123157828326},"8591735009847"]
["TECHNIK","VPC  4,8x680",null,"Vázací páska černá krátkodobě UV odolná, nosnost 22kg, průměr svazku 205mm, rozměr 4,8x680mm","100ks",14.39964965800832,{"$f":"F2516*(1-Elteq!$F$9)","v":14.39964965800832},"8591735019389"]
["TECHNIK","VPC  4,8x830",null,"Vázací páska černá krátkodobě UV odolná, nosnost 22kg, průměr svazku 250mm, rozměr 4,8x830mm","100ks",15.80992462451429,{"$f":"F2517*(1-Elteq!$F$9)","v":15.80992462451429},"8591735019396"]
["TECHNIK","VPC  7,6x150",null,"Vázací páska černá krátkodobě UV odolná, nosnost 54kg, průměr svazku 33mm, rozměr 7,6x150mm","100ks",3.7112499118578146,{"$f":"F2518*(1-Elteq!$F$9)","v":3.7112499118578146},"8591735016289"]
["TECHNIK","VPC  7,6x200",null,"Vázací páska černá krátkodobě UV odolná, nosnost 54kg, průměr svazku 50mm, rozměr 7,6x200mm","100ks",4.3421623968736434,{"$f":"F2519*(1-Elteq!$F$9)","v":4.3421623968736434},"8591735005139"]
["TECHNIK","VPC  7,6x240",null,"Vázací páska černá krátkodobě UV odolná, nosnost 54kg, průměr svazku 60mm, rozměr 7,6x240mm","100ks",4.8988498836523151,{"$f":"F2520*(1-Elteq!$F$9)","v":4.8988498836523151},"8591735016272"]
["TECHNIK","VPC  7,6x300",null,"Vázací páska černá krátkodobě UV odolná, nosnost 54kg, průměr svazku 76mm, rozměr 7,6x292mm","100ks",4.9730748818894712,{"$f":"F2521*(1-Elteq!$F$9)","v":4.9730748818894712},"8591735005146"]
["TECHNIK","VPC  7,6x370",null,"Vázací páska černá krátkodobě UV odolná, nosnost 54kg, průměr svazku 102mm, rozměr 7,6x368mm","100ks",5.1957498766009405,{"$f":"F2522*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735005153"]
["TECHNIK","VPC  7,6x370 UV",null,"Vázací páska černá dlouhodobě UV stabilní, nosnost 54kg, průměr svazku 102mm, rozměr 7,6x368mm","100ks",6.3091248501582848,{"$f":"F2523*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735050757"]
["TECHNIK","VPC  7,8x450",null,"Vázací páska černá krátkodobě UV odolná, nosnost 54kg, průměr svazku 125mm, rozměr 7,8x450mm","100ks",9.0925622840516453,{"$f":"F2524*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735005160"]
["TECHNIK","VPC  7,8x500",null,"Vázací páska černá krátkodobě UV odolná, nosnost 54kg, průměr svazku 138mm, rozměr 7,8x500mm","100ks",10.280162255846147,{"$f":"F2525*(1-Elteq!$F$9)","v":10.280162255846147},"8591735019495"]
["TECHNIK","VPC  7,8x550",null,"Vázací páska černá krátkodobě UV odolná, nosnost 54kg, průměr svazku 160mm, rozměr 7,8x550mm","100ks",10.354387254083303,{"$f":"F2526*(1-Elteq!$F$9)","v":10.354387254083303},"8591735005177"]
["TECHNIK","VPC  7,8x750",null,"Vázací páska černá krátkodobě UV odolná, nosnost 54kg, průměr svazku 216mm, rozměr 7,8x750mm","100ks",16.774849601597321,{"$f":"F2527*(1-Elteq!$F$9)","v":16.774849601597321},"8591735009748"]
["TECHNIK","VPC  9,0x 430",null,"Vázací páska černá krátkodobě UV odolná, nosnost 77kg, průměr svazku 125mm, rozměr 9,0x430mm","100ks",12.61824970031657,{"$f":"F2528*(1-Elteq!$F$9)","v":12.61824970031657},"8591735005191"]
["TECHNIK","VPC  9,0x 430 UV",null,"Vázací páska černá dlouhodobě UV stabilní, nosnost 77kg, průměr svazku 125mm, rozměr 9,0x430mm","100ks",15.030562143024149,{"$f":"F2529*(1-Elteq!$F$9)","v":15.030562143024149},"8591735054144"]
["TECHNIK","VPC  9,0x 530",null,"Vázací páska černá krátkodobě UV odolná, nosnost 77kg, průměr svazku 140mm, rozměr 9,0x530mm","100ks",15.216124638617039,{"$f":"F2530*(1-Elteq!$F$9)","v":15.216124638617039},"8591735005207"]
["TECHNIK","VPC  9,0x 760 D",null,"Vázací páska černá UV odolná s dvojitým zámkem, nosnost 55kg, průměr svazku 230mm, rozměr 9,0x760mm","100ks",45.280960174577196,{"$f":"F2531*(1-Elteq!$F$9)","v":45.280960174577196},"8591735056551"]
["TECHNIK","VPC  9,0x 780",null,"Vázací páska černá krátkodobě UV odolná, nosnost 77kg, průměr svazku 228mm, rozměr 9,0x775mm","100ks",17.81399957691751,{"$f":"F2532*(1-Elteq!$F$9)","v":17.81399957691751},"8591735005214"]
["TECHNIK","VPC  9,0x 920",null,"Vázací páska černá krátkodobě UV odolná, nosnost 77kg, průměr svazku 265mm, rozměr 9,0x920mm","100ks",29.393099301913892,{"$f":"F2533*(1-Elteq!$F$9)","v":29.393099301913892},"8591735053673"]
["TECHNIK","VPC  9,0x1020",null,"Vázací páska černá krátkodobě UV odolná, nosnost 77kg, průměr svazku 295mm, rozměr 9,0x1020mm","100ks",32.287874233162988,{"$f":"F2534*(1-Elteq!$F$9)","v":32.287874233162988},"8591735005221"]
["TECHNIK","VPC  9,0x1220",null,"Vázací páska černá krátkodobě UV odolná, nosnost 77kg, průměr svazku 352mm, rozměr 9,0x1220mm","100ks",46.019498907036898,{"$f":"F2535*(1-Elteq!$F$9)","v":46.019498907036898},"8591735007324"]
["TECHNIK","VPC  9,0x1530",null,"Vázací páska černá krátkodobě UV odolná, nosnost 77kg, průměr svazku 455mm, rozměr 9,0x1530mm","100ks",64.761310961918866,{"$f":"F2536*(1-Elteq!$F$9)","v":64.761310961918866},"8591735019402"]
["TECHNIK","VPC 13x 230",null,"Vázací páska černá krátkodobě UV odolná, nosnost 110kg, průměr svazku 50mm, rozměr 13x230mm","100ks",13.100712188858086,{"$f":"F2537*(1-Elteq!$F$9)","v":13.100712188858086},"8591735005283"]
["TECHNIK","VPC 13x 380",null,"Vázací páska černá krátkodobě UV odolná, nosnost 110kg, průměr svazku 96mm, rozměr 13x380mm","100ks",17.81399957691751,{"$f":"F2538*(1-Elteq!$F$9)","v":17.81399957691751},"8591735019419"]
["TECHNIK","VPC 13x 480",null,"Vázací páska černá krátkodobě UV odolná, nosnost 110kg, průměr svazku 121mm, rozměr 13x480mm","100ks",18.185124568103291,{"$f":"F2539*(1-Elteq!$F$9)","v":18.185124568103291},"8591735016210"]
["TECHNIK","VPC 13x 580",null,"Vázací páska černá krátkodobě UV odolná, nosnost 110kg, průměr svazku 140mm, rozměr 13x580mm","100ks",24.494249418261575,{"$f":"F2540*(1-Elteq!$F$9)","v":24.494249418261575},"8591735005290"]
["TECHNIK","VPC 13x 730",null,"Vázací páska černá krátkodobě UV odolná, nosnost 110kg, průměr svazku 200mm, rozměr 13x730mm","100ks",24.679811913854468,{"$f":"F2541*(1-Elteq!$F$9)","v":24.679811913854468},"8591735005306"]
["TECHNIK","VPC 13x 830",null,"Vázací páska černá krátkodobě UV odolná, nosnost 110kg, průměr svazku 219mm, rozměr 13x830mm","100ks",41.937124003993304,{"$f":"F2542*(1-Elteq!$F$9)","v":41.937124003993304},"8591735019426"]
["TECHNIK","VPC 13x1000",null,"Vázací páska černá krátkodobě UV odolná, nosnost 110kg, průměr svazku 300mm, rozměr 13x1000mm","100ks",42.308248995179085,{"$f":"F2543*(1-Elteq!$F$9)","v":42.308248995179085},"8591735005313"]
["TECHNIK","VPCDO 2,5x110",null,"Vázací páska černá do otvoru 2,5x110mm","1000ks",22.453061966739778,{"$f":"F2544*(1-Elteq!$F$9)","v":22.453061966739778},"8591735022358"]
["TECHNIK","VPCDO 3,6x150",null,"Vázací páska černá do otvoru 3,6x150mm","1000ks",22.638624462332668,{"$f":"F2545*(1-Elteq!$F$9)","v":22.638624462332668},"8591735022365"]
["TECHNIK","VPCDO 4,8x190",null,"Vázací páska černá do otvoru 4,8x190mm","1000ks",35.62799915383502,{"$f":"F2546*(1-Elteq!$F$9)","v":35.62799915383502},"8591735049898"]
["TECHNIK","VPCDO 4,8x200",null,"Vázací páska černá do otvoru 4,8x200mm","1000ks",39.710374056878614,{"$f":"F2547*(1-Elteq!$F$9)","v":39.710374056878614},"8591735022372"]
["TECHNIK","VPCDO 4,8x201",null,"Vázací páska černá do otvoru 4,8x201mm","100ks",5.9379998589725034,{"$f":"F2548*(1-Elteq!$F$9)","v":5.9379998589725034},"8591735049737"]
["TECHNIK","VPDO 2,5x110",null,"Vázací páska přírodní do otvoru 2,5x110mm - (aktuálně balení po 100ks)","1000ks",20.411874515217981,{"$f":"F2549*(1-Elteq!$F$9)","v":20.411874515217981},"8591735018245"]
["TECHNIK","VPDO 3,6x150",null,"Vázací páska přírodní do otvoru 3,6x150mm","1000ks",23.751999435890014,{"$f":"F2550*(1-Elteq!$F$9)","v":23.751999435890014},"8591735017842"]
["TECHNIK","VPDO 4,8x130",null,"Vázací páska přírodní do otvoru 4,8x130mm","1000ks",30.803374268419862,{"$f":"F2551*(1-Elteq!$F$9)","v":30.803374268419862},"8591735034412"]
["TECHNIK","VPDO 4,8x200",null,"Vázací páska přírodní do otvoru 4,8x200mm","1000ks",26.349874374190485,{"$f":"F2552*(1-Elteq!$F$9)","v":26.349874374190485},"8591735017859"]
["TECHNIK","VPSO 2,5x110",null,"Vázací páska přírodní 2,5x110mm s otvorem","100ks",2.2267499471146888,{"$f":"F2553*(1-Elteq!$F$9)","v":2.2267499471146888},"8591735034429"]
["TECHNIK","VPSO 3,6x150",null,"Vázací páska přírodní 3,6x150mm s otvorem","100ks",3.6370249136206585,{"$f":"F2554*(1-Elteq!$F$9)","v":3.6370249136206585},"8591735029654"]
["TECHNIK","VPSO 4,8x200",null,"Vázací páska přírodní 4,8x200mm s otvorem","100ks",6.3091248501582848,{"$f":"F2555*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735029364"]
["TECHNIK","VPSO 4,8x300",null,"Vázací páska přírodní 4,8x300mm s otvorem","100ks",14.510987155364054,{"$f":"F2556*(1-Elteq!$F$9)","v":14.510987155364054},"8591735029869"]
["TECHNIK","VPSO 4,8x370",null,"Vázací páska přírodní 4,8x370mm s otvorem","100ks",16.21816211481865,{"$f":"F2557*(1-Elteq!$F$9)","v":16.21816211481865},"8591735032197"]
["TECHNIK","VPSO 7,6x200",null,"Vázací páska přírodní 7,6x200mm s otvorem","100ks",11.467762227640646,{"$f":"F2558*(1-Elteq!$F$9)","v":11.467762227640646},"8591735032203"]
["TECHNIK","VPSO 7,6x300",null,"Vázací páska přírodní 7,6x300mm s otvorem","100ks",15.067674642142727,{"$f":"F2559*(1-Elteq!$F$9)","v":15.067674642142727},"8591735032210"]
["TECHNIK","VPSO 7,6x370",null,"Vázací páska přírodní 7,6x370mm s otvorem","100ks",17.888224575154666,{"$f":"F2560*(1-Elteq!$F$9)","v":17.888224575154666},"8591735032227"]
["TECHNIK","VPSO 7,9x400",null,"Vázací páska přírodní 7,9x400mm s otvorem","100ks",32.25076173404441,{"$f":"F2561*(1-Elteq!$F$9)","v":32.25076173404441},"8591735034436"]
["TECHNIK","VPŽDO 2,5x110",null,"Vázací páska žlutá do otvoru 2,5x110mm","1000ks",22.453061966739778,{"$f":"F2562*(1-Elteq!$F$9)","v":22.453061966739778},"8591735032234"]
["TECHNIK","BP 48x66 bílá",null,"Balicí páska samolepící, 48mm x 66m, barva bílá bez potisku","1ks",0.85358747972729732,{"$f":"F2563*(1-Elteq!$F$9)","v":0.85358747972729732},""]
["TECHNIK","BP 48x66 bílá KŘEHKÉ",null,"Balicí páska samolepící, 48mm x 66m, barva bílá s potiskem KŘEHKÉ","1ks",1.6700624603360166,{"$f":"F2564*(1-Elteq!$F$9)","v":1.6700624603360166},""]
["TECHNIK","BP 48x66 hnědá",null,"Balicí páska samolepící, 48mm x 66m, barva hnědá bez potisku","1ks",0.81647498060871926,{"$f":"F2565*(1-Elteq!$F$9)","v":0.81647498060871926},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"BP 48x66 transp",null,"Balicí páska samolepící, 48mm x 66m, barva transparentní bez potisku","1ks",0.81647498060871926,{"$f":"F2566*(1-Elteq!$F$9)","v":0.81647498060871926},""]
["TECHNIK","EP 15x10 bílá",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x15mm/10m, použití +10°C až +85°C, bílá","10ks",1.8185124568103292,{"$f":"F2567*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735041205"]
["TECHNIK","EP 15x10 color",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x15mm/10m, použití +10°C až +85°C, různé barvy","10ks",1.8556249559289073,{"$f":"F2568*(1-Elteq!$F$9)","v":1.8556249559289073},"8591735041212"]
["TECHNIK","EP 15x10 černá",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x15mm/10m, použití +10°C až +85°C, černá","10ks",1.8185124568103292,{"$f":"F2569*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735041229"]
["TECHNIK","EP 15x10 fialová",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x15mm/10m, použití +10°C až +85°C, fialová","10ks",1.8185124568103292,{"$f":"F2570*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735041236"]
["TECHNIK","EP 15x10 hnědá",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x15mm/10m, použití +10°C až +85°C, hnědá","10ks",1.8185124568103292,{"$f":"F2571*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735041243"]
["TECHNIK","EP 15x10 rudá",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x15mm/10m, použití +10°C až +85°C, rudá","10ks",1.8185124568103292,{"$f":"F2572*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735041250"]
["TECHNIK","EP 15x10 sv.modrá",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x15mm/10m, použití +10°C až +85°C, světle modrá","10ks",1.8185124568103292,{"$f":"F2573*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735041267"]
["TECHNIK","EP 15x10 šedá",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x15mm/10m, použití +10°C až +85°C, šedá","10ks",1.8185124568103292,{"$f":"F2574*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735041274"]
["TECHNIK","EP 15x10 tm.modrá",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x15mm/10m, použití +10°C až +85°C, tmavě modrá","10ks",1.8185124568103292,{"$f":"F2575*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735041281"]
["TECHNIK","EP 15x10 zelená",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x15mm/10m, použití +10°C až +85°C, zelená","10ks",1.8185124568103292,{"$f":"F2576*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735041298"]
["TECHNIK","EP 15x10 žlutá",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x15mm/10m, použití +10°C až +85°C, žlutá","10ks",1.8185124568103292,{"$f":"F2577*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735041304"]
["TECHNIK","EP 15x10 žz",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x15mm/10m, použití +10°C až +85°C, žluto-zelená","10ks",1.8185124568103292,{"$f":"F2578*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735041311"]
["TECHNIK","EP 15x20.SF bílá",null,"Elektroizolační páska samolepící PVC profesionální 0,19x15mm/20m, použití -10°C až +85°C, bílá","10ks",8.1647498060871921,{"$f":"F2579*(1-Elteq!$F$9)","v":8.1647498060871921},"8591735042820"]
["TECHNIK","EP 15x20.SF černá",null,"Elektroizolační páska samolepící PVC profesionální 0,19x15mm/20m, použití -10°C až +85°C, černá","10ks",8.1647498060871921,{"$f":"F2580*(1-Elteq!$F$9)","v":8.1647498060871921},"8591735042837"]
["TECHNIK","EP 15x20.SF fialová",null,"Elektroizolační páska samolepící PVC profesionální 0,19x15mm/20m, použití -10°C až +85°C, fialová","10ks",8.1647498060871921,{"$f":"F2581*(1-Elteq!$F$9)","v":8.1647498060871921},"8591735043834"]
["TECHNIK","EP 15x20.SF hnědá",null,"Elektroizolační páska samolepící PVC profesionální 0,19x15mm/20m, použití -10°C až +85°C, hnědá","10ks",8.1647498060871921,{"$f":"F2582*(1-Elteq!$F$9)","v":8.1647498060871921},"8591735043827"]
["TECHNIK","EP 15x20.SF modrá",null,"Elektroizolační páska samolepící PVC profesionální 0,19x15mm/20m, použití -10°C až +85°C, modrá","10ks",8.1647498060871921,{"$f":"F2583*(1-Elteq!$F$9)","v":8.1647498060871921},"8591735042851"]
["TECHNIK","EP 15x20.SF rudá",null,"Elektroizolační páska samolepící PVC profesionální 0,19x15mm/20m, použití -10°C až +85°C, rudá","10ks",8.1647498060871921,{"$f":"F2584*(1-Elteq!$F$9)","v":8.1647498060871921},"8591735042844"]
["TECHNIK","EP 15x20.SF šedá",null,"Elektroizolační páska samolepící PVC profesionální 0,19x15mm/20m, použití -10°C až +85°C, šedá","10ks",8.1647498060871921,{"$f":"F2585*(1-Elteq!$F$9)","v":8.1647498060871921},"8591735042868"]
["TECHNIK","EP 15x20.SF zelená",null,"Elektroizolační páska samolepící PVC profesionální 0,19x15mm/20m, použití -10°C až +85°C, zelená","10ks",8.1647498060871921,{"$f":"F2586*(1-Elteq!$F$9)","v":8.1647498060871921},"8591735043841"]
["TECHNIK","EP 15x20.SF žlutá",null,"Elektroizolační páska samolepící PVC profesionální 0,19x15mm/20m, použití -10°C až +85°C, žlutá","10ks",8.1647498060871921,{"$f":"F2587*(1-Elteq!$F$9)","v":8.1647498060871921},"8591735043858"]
["TECHNIK","EP 19x18 MV černá",null,"Elektroizolační páska samolepící PVC mrazuvzdorná 0,18x19mm/18m použití -18°C až +105°C, černá","1ks",1.6700624603360166,{"$f":"F2588*(1-Elteq!$F$9)","v":1.6700624603360166},""]
["TECHNIK","EP 19x20 bílá",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x19mm/20m, použití +10°C až +85°C, bílá","10ks",5.1957498766009405,{"$f":"F2589*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735048310"]
["TECHNIK","EP 19x20 color",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x19mm/20m, použití +10°C až +85°C, různé barvy","10ks",5.1957498766009405,{"$f":"F2590*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735054489"]
["TECHNIK","EP 19x20 černá",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x19mm/20m, použití +10°C až +85°C, černá","10ks",5.1957498766009405,{"$f":"F2591*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735046019"]
["TECHNIK","EP 19x20 modrá",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x19mm/20m, použití +10°C až +85°C, modrá","10ks",5.1957498766009405,{"$f":"F2592*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735048358"]
["TECHNIK","EP 19x20 rudá",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x19mm/20m, použití +10°C až +85°C, rudá","10ks",5.1957498766009405,{"$f":"F2593*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735048327"]
["TECHNIK","EP 19x20 šedá",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x19mm/20m, použití +10°C až +85°C, šedá","10ks",5.1957498766009405,{"$f":"F2594*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735047269"]
["TECHNIK","EP 19x20 zelená",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x19mm/20m, použití +10°C až +85°C, zelená","10ks",5.1957498766009405,{"$f":"F2595*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735048334"]
["TECHNIK","EP 19x20 žlutá",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x19mm/20m, použití +10°C až +85°C, žlutá","10ks",5.1957498766009405,{"$f":"F2596*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735048341"]
["TECHNIK","EP 19x20 žz",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x19mm/20m, použití +10°C až +85°C, žluto-zelená","10ks",5.1957498766009405,{"$f":"F2597*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735046002"]
["TECHNIK","EP 19x20.SF bílá",null,"Elektroizolační páska samolepící PVC profesionální 0,19x19mm/20m, použití -10°C až +85°C, bílá","10ks",10.020374762016099,{"$f":"F2598*(1-Elteq!$F$9)","v":10.020374762016099},"8591735043865"]
["TECHNIK","EP 19x20.SF černá",null,"Elektroizolační páska samolepící PVC profesionální 0,19x19mm/20m, použití -10°C až +85°C, černá","10ks",10.020374762016099,{"$f":"F2599*(1-Elteq!$F$9)","v":10.020374762016099},"8591735042875"]
["TECHNIK","EP 19x20.SF modrá",null,"Elektroizolační páska samolepící PVC profesionální 0,19x19mm/20m, použití -10°C až +85°C, modrá","10ks",10.020374762016099,{"$f":"F2600*(1-Elteq!$F$9)","v":10.020374762016099},"8591735043896"]
["TECHNIK","EP 19x20.SF rudá",null,"Elektroizolační páska samolepící PVC profesionální 0,19x19mm/20m, použití -10°C až +85°C, rudá","10ks",10.020374762016099,{"$f":"F2601*(1-Elteq!$F$9)","v":10.020374762016099},"8591735043889"]
["TECHNIK","EP 19x20.SF zelená",null,"Elektroizolační páska samolepící PVC profesionální 0,19x19mm/20m, použití -10°C až +85°C, zelená","10ks",10.020374762016099,{"$f":"F2602*(1-Elteq!$F$9)","v":10.020374762016099},"8591735043872"]
["TECHNIK","EP 19x20.SF žlutá",null,"Elektroizolační páska samolepící PVC profesionální 0,19x19mm/20m, použití -10°C až +85°C, žlutá","10ks",10.020374762016099,{"$f":"F2603*(1-Elteq!$F$9)","v":10.020374762016099},"8591735042882"]
["TECHNIK","EP 25x18 MV černá",null,"Elektroizolační páska samolepící PVC mrazuvzdorná 0,18x25mm/18m použití -18°C až +105°C, černá","1ks",2.1154124497589541,{"$f":"F2604*(1-Elteq!$F$9)","v":2.1154124497589541},""]
["TECHNIK","EP 25x20 černá",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x25mm/20m, použití +10°C až +85°C, černá","1ks",0.66802498413440659,{"$f":"F2605*(1-Elteq!$F$9)","v":0.66802498413440659},""]
["TECHNIK","EP 25x20 žz",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x25mm/20m, použití +10°C až +85°C, žluto-zelená","1ks",0.66802498413440659,{"$f":"F2606*(1-Elteq!$F$9)","v":0.66802498413440659},""]
["TECHNIK","EP 25x20.SF bílá",null,"Elektroizolační páska samolepící PVC profesionální 0,19x25mm/20m, použití -10°C až +85°C, bílá","1ks",1.3360499682688132,{"$f":"F2607*(1-Elteq!$F$9)","v":1.3360499682688132},"8591735042899"]
["TECHNIK","EP 25x20.SF černá",null,"Elektroizolační páska samolepící PVC profesionální 0,19x25mm/20m, použití -10°C až +85°C, černá","1ks",1.3360499682688132,{"$f":"F2608*(1-Elteq!$F$9)","v":1.3360499682688132},"8591735042905"]
["TECHNIK","EP 25x20.SF modrá",null,"Elektroizolační páska samolepící PVC profesionální 0,19x25mm/20m, použití -10°C až +85°C, modrá","1ks",1.3360499682688132,{"$f":"F2609*(1-Elteq!$F$9)","v":1.3360499682688132},"8591735042912"]
["TECHNIK","EP 25x20.SF rudá",null,"Elektroizolační páska samolepící PVC profesionální 0,19x25mm/20m, použití -10°C až +85°C, rudá","1ks",1.3360499682688132,{"$f":"F2610*(1-Elteq!$F$9)","v":1.3360499682688132},"8591735042929"]
["TECHNIK","EP 38x20 černá",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x38mm/20m, použití +10°C až +85°C, černá","1ks",1.00203747620161,{"$f":"F2611*(1-Elteq!$F$9)","v":1.00203747620161},""]
["TECHNIK","EP 38x20.SF černá",null,"Elektroizolační páska samolepící PVC profesionální 0,19x38mm/20m, použití -10°C až +85°C, černá","1ks",2.00407495240322,{"$f":"F2612*(1-Elteq!$F$9)","v":2.00407495240322},"8591735048594"]
["TECHNIK","EP 45x 5 HELP",null,"Elektroizolační páska samolepící pro všestranné použití, 45mm/5m, od -40°C do +80°C, různé barvy","12ks",12.432687204723679,{"$f":"F2613*(1-Elteq!$F$9)","v":12.432687204723679},"8591735041434"]
["TECHNIK","EP 50x10 černá",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x50mm/10m, použití +10°C až +85°C, černá","1ks",0.66802498413440659,{"$f":"F2614*(1-Elteq!$F$9)","v":0.66802498413440659},""]
["TECHNIK","EP 50x20 černá",null,"Elektroizolační páska samolepící PVC, rozměr 0,13x50mm/20m, použití +10°C až +85°C, černá","1ks",1.3360499682688132,{"$f":"F2615*(1-Elteq!$F$9)","v":1.3360499682688132},""]
["TECHNIK","EP 50x20.SF bílá",null,"Elektroizolační páska samolepící PVC profesionální 0,19x50mm/20m, použití -10°C až +85°C, bílá","1ks",2.6349874374190483,{"$f":"F2616*(1-Elteq!$F$9)","v":2.6349874374190483},"8591735043902"]
["TECHNIK","EP 50x20.SF černá",null,"Elektroizolační páska samolepící PVC profesionální 0,19x50mm/20m, použití -10°C až +85°C, černá","1ks",2.6349874374190483,{"$f":"F2617*(1-Elteq!$F$9)","v":2.6349874374190483},"8591735042936"]
["TECHNIK","EP 50x20.SF modrá",null,"Elektroizolační páska samolepící PVC profesionální 0,19x50mm/20m, použití -10°C až +85°C, modrá","1ks",2.6349874374190483,{"$f":"F2618*(1-Elteq!$F$9)","v":2.6349874374190483},"8591735042943"]
["TECHNIK","EP 701-40/50x10",null,"Plastická páska protikorozní ochrany 50mm x 10m pro izolaci spojek bleskosvodů a uzemnění","1ks",8.5358747972729727,{"$f":"F2619*(1-Elteq!$F$9)","v":8.5358747972729727},""]
["TECHNIK","EP3M 15x10 černá",null,"Elektroizolační páska samolepící PVC, 3M Temflex 1500, 15mm/10m, použití do +90°C, barva černá","1ks",0.63091248501582853,{"$f":"F2620*(1-Elteq!$F$9)","v":0.63091248501582853},""]
["TECHNIK","EP3M 15x10 modrá",null,"Elektroizolační páska samolepící PVC, 3M Temflex 1500, 15mm/10m, použití do +90°C, barva modrá","1ks",0.63091248501582853,{"$f":"F2621*(1-Elteq!$F$9)","v":0.63091248501582853},""]
["TECHNIK","EP3M 15x10 rudá",null,"Elektroizolační páska samolepící PVC, 3M Temflex 1500, 15mm/10m, použití do +90°C, barva rudá","1ks",0.63091248501582853,{"$f":"F2622*(1-Elteq!$F$9)","v":0.63091248501582853},""]
["TECHNIK","EP3M 15x10 zelená",null,"Elektroizolační páska samolepící PVC, 3M Temflex 1500, 15mm/10m, použití do +90°C, barva zelená","1ks",1.0762624744387663,{"$f":"F2623*(1-Elteq!$F$9)","v":1.0762624744387663},""]
["TECHNIK","EP3M 15x10 žz",null,"Elektroizolační páska samolepící PVC, 3M Temflex 1500, 15mm/10m, použit do +90°C, barva žluto-zelená","1ks",0.63091248501582853,{"$f":"F2624*(1-Elteq!$F$9)","v":0.63091248501582853},""]
["TECHNIK","EP3M 19x20 černá",null,"Elektroizolační páska samolepící PVC, 3M 19mm/20m, barva černá UV od -18°C, Scotch Super 33+","1ks",7.4596123228342073,{"$f":"F2625*(1-Elteq!$F$9)","v":7.4596123228342073},""]
["TECHNIK","EP3M 19x20 rudá",null,"Elektroizolační páska samolepící PVC, 3M Temflex 1500, 19mm/20m, použití do +90°C, barva rudá","1ks",1.3731624673873914,{"$f":"F2626*(1-Elteq!$F$9)","v":1.3731624673873914},""]
["TECHNIK","EP3M 19x33 typ 69",null,"Páska ze skelné tkaniny, samozhášivá se silikonovým lepidlem pro vysokoteplotní aplikace do +190°C","1ks",38.485661585965538,{"$f":"F2627*(1-Elteq!$F$9)","v":38.485661585965538},"8591735040192"]
["TECHNIK","EP3M 19x9,1 černá",null,"Elektroizolační páska samolepící gumová, 19mm/9,1m, barva černá UV, 3M Scotch 23 pro VN do 69kV","1ks",13.583174677399601,{"$f":"F2628*(1-Elteq!$F$9)","v":13.583174677399601},""]
["TECHNIK","EP3M 25x7 černá",null,"Elektroizolační páska EPR pro VN do 69kV, 0,75x25mm/7m, barva černá UV, 3M Scotch 23","1ks",13.620287176518179,{"$f":"F2629*(1-Elteq!$F$9)","v":13.620287176518179},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"EP3M 25x9,1 černá",null,"Elektroizolační páska EPR pro VN do 69kV, 0,75x25mm/9,1m, barva černá UV, 3M Scotch 23","1ks",16.329499612174384,{"$f":"F2630*(1-Elteq!$F$9)","v":16.329499612174384},""]
["TECHNIK","EP3M 38x33 černá",null,"Elektroizolační páska samolepící PVC, 38mm/33m, barva černá UV od -18°C, 3M Scotch Super 33+","1ks",18.185124568103291,{"$f":"F2631*(1-Elteq!$F$9)","v":18.185124568103291},""]
["TECHNIK","EPAL 50x50",null,"Hliníková samolepicí páska rozměr 50mm x 50m","1ks",5.4555373704309877,{"$f":"F2632*(1-Elteq!$F$9)","v":5.4555373704309877},""]
["TECHNIK","EPT 25x9 šedá",null,"Textilní páska samolepicí 19mm x 9m, potažená PE, použití do +90°C, šedostříbrná DUCT","1ks",0.74224998237156292,{"$f":"F2633*(1-Elteq!$F$9)","v":0.74224998237156292},""]
["TECHNIK","EPV  50x33 žl-černá",null,"Výstražná páska samolepicí PVC, 50mm x 33m, barva žluto-černá","1ks",5.3070873739566746,{"$f":"F2634*(1-Elteq!$F$9)","v":5.3070873739566746},"8591735052898"]
["TECHNIK","TFL 12x10",null,"Teflonová páska 12mm x 10m x 0,075mm, barva bílá (10ks)","10ks",4.0823749030435961,{"$f":"F2635*(1-Elteq!$F$9)","v":4.0823749030435961},""]
["TECHNIK","VFP  80x100 žl-černá",null,"Výstražná fólie PVC, 80mm x 100m, barva žluto-černá","1ks",2.9689999294862517,{"$f":"F2636*(1-Elteq!$F$9)","v":2.9689999294862517},"8591735049850"]
["TECHNIK","VFP 100x100 žl-černá",null,"Výstražná fólie PVC, 100mm x 100m, barva žluto-černá","1ks",3.1545624250791424,{"$f":"F2637*(1-Elteq!$F$9)","v":3.1545624250791424},"8591735049867"]
["TECHNIK","VULK 19x3,5 NN",null,"Samovulkanizační PIB páska 19mm x 3,5m, barva černá, -40 až +90°C, proti vlhkosti, protažení 600%","1ks",1.8556249559289073,{"$f":"F2638*(1-Elteq!$F$9)","v":1.8556249559289073},"8591735042752"]
["TECHNIK","VULK 19x7,5",null,"Samovulkanizační PE páska 19mm x 7,5m, barva černá, -34 až +85°C, UV odolná, protažení 10%","1ks",3.1174499259605644,{"$f":"F2639*(1-Elteq!$F$9)","v":3.1174499259605644},"8591735042790"]
["TECHNIK","VULK 19x7,5 NN",null,"Samovulkanizační PIB páska 19mm x 7,5m, barva černá, -40 až +90°C, proti vlhkosti, protažení 600%","1ks",3.3030124215534551,{"$f":"F2640*(1-Elteq!$F$9)","v":3.3030124215534551},"8591735042769"]
["TECHNIK","VULK 25x10 NN",null,"Samovulkanizační PIB páska 25mm x 10m, barva černá, -40 až +90°C, proti vlhkosti, protažení 600%","1ks",3.7112499118578146,{"$f":"F2641*(1-Elteq!$F$9)","v":3.7112499118578146},"8591735049812"]
["TECHNIK","VULK 25x5 NN",null,"Samovulkanizační PIB páska 25mm x 5m, barva černá, -40 až +90°C, proti vlhkosti, protažení 600%","1ks",1.9298499541660636,{"$f":"F2642*(1-Elteq!$F$9)","v":1.9298499541660636},"8591735042776"]
["TECHNIK","VULK 25x7,5",null,"Samovulkanizační PE páska 25mm x 7,5m, barva černá, -34 až +85°C, UV odolná, protažení 10%","1ks",4.00814990480644,{"$f":"F2643*(1-Elteq!$F$9)","v":4.00814990480644},"8591735042806"]
["TECHNIK","VULK 25x7,5 NN",null,"Samovulkanizační PIB páska 25mm x 7,5m, barva černá, -40 až +90°C, proti vlhkosti, protažení 600%","1ks",4.0823749030435961,{"$f":"F2644*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735042783"]
["TECHNIK","VULK 50x7,5",null,"Samovulkanizační PE páska 50mm x 7,5m, barva černá, -34 až +85°C, UV odolná, protažení 10%","1ks",7.7936248149014107,{"$f":"F2645*(1-Elteq!$F$9)","v":7.7936248149014107},"8591735042813"]
["TECHNIK","VULK 50x7,5 NN",null,"Samovulkanizační PIB páska 50mm x 7,5m, barva černá, -40 až +90°C, proti vlhkosti, protažení 600%","1ks",7.6080623193085195,{"$f":"F2646*(1-Elteq!$F$9)","v":7.6080623193085195},"8591735049874"]
["TECHNIK","PP NIT  50",null,"Ruční pojistná nit délka 50mm","5000ks",31.731186746384314,{"$f":"F2647*(1-Elteq!$F$9)","v":31.731186746384314},""]
["TECHNIK","PP NIT  75",null,"Ruční pojistná nit délka 75mm","5000ks",20.782999506403762,{"$f":"F2648*(1-Elteq!$F$9)","v":20.782999506403762},"8591735017347"]
["TECHNIK","PP NIT 125",null,"Ruční pojistná nit délka 125mm","5000ks",21.896374479961107,{"$f":"F2649*(1-Elteq!$F$9)","v":21.896374479961107},"8591735017972"]
["TECHNIK","PP NIT 175",null,"Ruční pojistná nit délka 175mm","5000ks",23.009749453518449,{"$f":"F2650*(1-Elteq!$F$9)","v":23.009749453518449},"8591735052058"]
["TECHNIK","PP NIT 225",null,"Ruční pojistná nit délka 225mm","5000ks",24.123124427075794,{"$f":"F2651*(1-Elteq!$F$9)","v":24.123124427075794},"8591735052065"]
["TECHNIK","VPK 100",null,"Páska kuličková přírodní, nosnost do 8kg, délka 100mm","100ks",1.00203747620161,{"$f":"F2652*(1-Elteq!$F$9)","v":1.00203747620161},"8591735013349"]
["TECHNIK","VPK 120",null,"Páska kuličková přírodní, nosnost do 8kg, délka 120mm","100ks",1.8185124568103292,{"$f":"F2653*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735018221"]
["TECHNIK","VPK 150",null,"Páska kuličková přírodní, nosnost do 10kg, délka 150mm","100ks",3.2287874233162985,{"$f":"F2654*(1-Elteq!$F$9)","v":3.2287874233162985},"8591735005399"]
["TECHNIK","VPK 180",null,"Páska kuličková přírodní, nosnost do 12kg, délka 180mm","100ks",4.861737384533737,{"$f":"F2655*(1-Elteq!$F$9)","v":4.861737384533737},"8591735018238"]
["TECHNIK","VPK 226",null,"Páska kuličková přírodní, nosnost do 14kg, délka 226mm","100ks",7.6080623193085195,{"$f":"F2656*(1-Elteq!$F$9)","v":7.6080623193085195},"8591735005573"]
["TECHNIK","VPK 280",null,"Páska kuličková přírodní, nosnost do 22kg, délka 280mm","100ks",8.7214372928658648,{"$f":"F2657*(1-Elteq!$F$9)","v":8.7214372928658648},"8591735009908"]
["TECHNIK","VPKC 100",null,"Páska kuličková černá UV odolná, nosnost do 8kg, délka 100mm","100ks",1.1504874726759224,{"$f":"F2658*(1-Elteq!$F$9)","v":1.1504874726759224},"8591735056247"]
["TECHNIK","VPKC 120",null,"Páska kuličková černá UV odolná, nosnost do 8kg, délka 120mm","100ks",2.1154124497589541,{"$f":"F2659*(1-Elteq!$F$9)","v":2.1154124497589541},"8591735056087"]
["TECHNIK","VPKC 150",null,"Páska kuličková černá UV odolná, nosnost do 10kg, délka 150mm","100ks",3.7112499118578146,{"$f":"F2660*(1-Elteq!$F$9)","v":3.7112499118578146},"8591735022341"]
["TECHNIK","VPKC 180",null,"Páska kuličková černá UV odolná, nosnost do 12kg, délka 180mm","100ks",5.6039873669053,{"$f":"F2661*(1-Elteq!$F$9)","v":5.6039873669053},"8591735056254"]
["TECHNIK","VPKC 226",null,"Páska kuličková černá UV odolná, nosnost do 14kg, délka 226mm","100ks",8.7214372928658648,{"$f":"F2662*(1-Elteq!$F$9)","v":8.7214372928658648},"8591735056094"]
["TECHNIK","VPKC 280",null,"Páska kuličková černá UV odolná, nosnost do 22kg, délka 280mm","100ks",10.020374762016099,{"$f":"F2663*(1-Elteq!$F$9)","v":10.020374762016099},"8591735056100"]
["TECHNIK","VPM 2,5x100 sv.modrá",null,"Vázací páska metalizovaná s 10% obsahem kovu, sv. modrá do 8kg, rozměr 2,5x100mm","100ks",20.040749524032197,{"$f":"F2664*(1-Elteq!$F$9)","v":20.040749524032197},"8591735036393"]
["TECHNIK","VPM 3,4x200 sv.modrá",null,"Vázací páska metalizovaná s 10% obsahem kovu, sv. modrá do 18kg, rozměr 3,4x200mm","100ks",25.42206189622603,{"$f":"F2665*(1-Elteq!$F$9)","v":25.42206189622603},"8591735036409"]
["TECHNIK","VPM 4,8x190 sv.modrá",null,"Vázací páska metalizovaná s 10% obsahem kovu, sv. modrá do 22kg, rozměr 4,8x200mm","100ks",27.277686852154936,{"$f":"F2666*(1-Elteq!$F$9)","v":27.277686852154936},"8591735036065"]
["TECHNIK","VPM 4,8x290 sv.modrá",null,"Vázací páska metalizovaná s 10% obsahem kovu, sv. modrá do 22kg, rozměr 4,8x290mm","100ks",47.689561367372917,{"$f":"F2667*(1-Elteq!$F$9)","v":47.689561367372917},"8591735034337"]
["TECHNIK","VPM 4,8x370 sv.modrá",null,"Vázací páska metalizovaná s 10% obsahem kovu, sv. modrá do 22kg, rozměr 4,8x370mm","100ks",52.514186252788079,{"$f":"F2668*(1-Elteq!$F$9)","v":52.514186252788079},"8591735036416"]
["TECHNIK","VPM 7,6x370 sv.modrá",null,"Vázací páska metalizovaná s 10% obsahem kovu, sv. modrá do 54kg, rozměr 7,6x370mm","100ks",54.555373704309872,{"$f":"F2669*(1-Elteq!$F$9)","v":54.555373704309872},"8591735050016"]
["TECHNIK","VPZIP 13x150",null,"Páska svazkovací se suchým zipem oboustranná, šíře 13mm, délka 150mm, barva černá","100ks",23.677774437652857,{"$f":"F2670*(1-Elteq!$F$9)","v":23.677774437652857},"8591735045333"]
["TECHNIK","VPZIP 13x200 bílá",null,"Páska svazkovací se suchým zipem oboustranná, šíře 13mm, délka 200mm, barva bílá (balení 50ks)","50ks",16.03259961922576,{"$f":"F2671*(1-Elteq!$F$9)","v":16.03259961922576},"8591735055820"]
["TECHNIK","VPZIP 13x200 černá",null,"Páska svazkovací se suchým zipem oboustranná, šíře 13mm, délka 200mm, barva černá","100ks",28.391061825712281,{"$f":"F2672*(1-Elteq!$F$9)","v":28.391061825712281},"8591735045340"]
["TECHNIK","VPZIP 13x200 modrá",null,"Páska svazkovací se suchým zipem oboustranná, šíře 13mm, délka 200mm, barva černá (balení 50ks)","50ks",16.03259961922576,{"$f":"F2673*(1-Elteq!$F$9)","v":16.03259961922576},"8591735055813"]
["TECHNIK","VPZIP 13x200 rudá",null,"Páska svazkovací se suchým zipem oboustranná, šíře 13mm, délka 200mm, barva červená (balení 50ks)","50ks",16.03259961922576,{"$f":"F2674*(1-Elteq!$F$9)","v":16.03259961922576},"8591735055509"]
["TECHNIK","VPZIP 13x250",null,"Páska svazkovací se suchým zipem oboustranná, šíře 13mm, délka 250mm, barva černá","100ks",36.333136637088003,{"$f":"F2675*(1-Elteq!$F$9)","v":36.333136637088003},"8591735045357"]
["TECHNIK","VPZIP 20x300",null,"Páska svazkovací se suchým zipem oboustranná, šíře 20mm, délka 300mm, barva černá ","100ks",47.763786365610073,{"$f":"F2676*(1-Elteq!$F$9)","v":47.763786365610073},"8591735045364"]
["TECHNIK","VPZIP 30x400",null,"Páska svazkovací se suchým zipem oboustranná, šíře 30mm, délka 400mm, barva černá ","100ks",56.336773662001626,{"$f":"F2677*(1-Elteq!$F$9)","v":56.336773662001626},"8591735045371"]
["TECHNIK","VPZIP 30x600",null,"Páska svazkovací se suchým zipem oboustranná, šíře 30mm, délka 600mm, barva černá","100ks",64.909760958393178,{"$f":"F2678*(1-Elteq!$F$9)","v":64.909760958393178},"8591735045388"]
["TECHNIK","VPZIP-100",null,"Páska svazkovací se suchým zipem oboustranná, šíře 100mm, barva černá (cívka 25m)","25m",127.66699696790882,{"$f":"F2679*(1-Elteq!$F$9)","v":127.66699696790882},"8591735054014"]
["TECHNIK","VPZIP-12",null,"Páska svazkovací se suchým zipem oboustranná, šíře 12mm, barva černá (cívka 25m)","25m",15.587249629802821,{"$f":"F2680*(1-Elteq!$F$9)","v":15.587249629802821},"8591735032241"]
["TECHNIK","VPZIP-20",null,"Páska svazkovací se suchým zipem oboustranná, šíře 20mm, barva černá (cívka 25m)","25m",28.205499330119391,{"$f":"F2681*(1-Elteq!$F$9)","v":28.205499330119391},"8591735036553"]
["TECHNIK","VPZIP-20 S",null,"Páska svazkovací se suchým zipem oboustranná, šíře 20mm, barva černá (cívka 25m) samozhášivá","25m",50.361661303910545,{"$f":"F2682*(1-Elteq!$F$9)","v":50.361661303910545},""]
["TECHNIK","VPZIP-25",null,"Páska svazkovací se suchým zipem oboustranná, šíře 25mm, barva černá (cívka 25m)","25m",30.246686781641188,{"$f":"F2683*(1-Elteq!$F$9)","v":30.246686781641188},"8591735032258"]
["TECHNIK","VPZIP-50",null,"Páska svazkovací se suchým zipem oboustranná, šíře 50mm, barva černá (cívka 25m)","25m",59.008873598539253,{"$f":"F2684*(1-Elteq!$F$9)","v":59.008873598539253},"8591735032265"]
["TECHNIK","VPN  2,5x100",null,"Vázací páska nehořlavá (potlačující hoření V0) nosnost   8kg, průměr svazku 22mm, rozměr 2,5x100mm","100ks",0.92781247796445365,{"$f":"F2685*(1-Elteq!$F$9)","v":0.92781247796445365},"8591735034443"]
["TECHNIK","VPN  2,5x160",null,"Vázací páska nehořlavá (potlačující hoření V0) nosnost   8kg, průměr svazku 40mm, rozměr 2,5x160mm","100ks",1.6700624603360166,{"$f":"F2686*(1-Elteq!$F$9)","v":1.6700624603360166},"8591735053284"]
["TECHNIK","VPN  3,6x150",null,"Vázací páska nehořlavá (potlačující hoření V0) nosnost 13kg, průměr svazku 35mm, rozměr 3,6x150mm","100ks",2.00407495240322,{"$f":"F2687*(1-Elteq!$F$9)","v":2.00407495240322},"8591735034450"]
["TECHNIK","VPN  3,6x200",null,"Vázací páska nehořlavá (potlačující hoření V0) nosnost 13kg, průměr svazku 53mm, rozměr 3,6x200mm","100ks",2.783437433893361,{"$f":"F2688*(1-Elteq!$F$9)","v":2.783437433893361},"8591735034467"]
["TECHNIK","VPN  3,6x290",null,"Vázací páska nehořlavá (potlačující hoření V0) nosnost 13kg, průměr svazku 75mm, rozměr 3,6x290mm","100ks",5.1957498766009405,{"$f":"F2689*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735034474"]
["TECHNIK","VPN  4,8x200",null,"Vázací páska nehořlavá (potlačující hoření V0) nosnost 22kg, průměr svazku 50mm, rozměr 4,8x200mm","100ks",3.8968124074507053,{"$f":"F2690*(1-Elteq!$F$9)","v":3.8968124074507053},"8591735034481"]
["TECHNIK","VPN  4,8x300",null,"Vázací páska nehořlavá (potlačující hoření V0) nosnost 22kg, průměr svazku 76mm, rozměr 4,8x300mm","100ks",5.5668748677867219,{"$f":"F2691*(1-Elteq!$F$9)","v":5.5668748677867219},"8591735054311"]
["TECHNIK","VPN  4,8x370",null,"Vázací páska nehořlavá (potlačující hoření V0) nosnost 22kg, průměr svazku 102mm, rozměr 4,8x368mm","100ks",9.0925622840516453,{"$f":"F2692*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735034498"]
["TECHNIK","VPST 4,5x 100",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 45kg, průměr svazku 22mm, rozměr 4,5x100x0,3mm","100ks",19.298499541660636,{"$f":"F2693*(1-Elteq!$F$9)","v":19.298499541660636},"8591735049683"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"VPST 4,5x 127",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 45kg, průměr svazku 28mm, rozměr 4,5x127x0,3mm","100ks",19.855187028439307,{"$f":"F2694*(1-Elteq!$F$9)","v":19.855187028439307},"8591735046460"]
["TECHNIK","VPST 4,5x 152",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 45kg, průměr svazku 35mm, rozměr 4,5x152x0,3mm","100ks",21.710811984368217,{"$f":"F2695*(1-Elteq!$F$9)","v":21.710811984368217},"8591735019518"]
["TECHNIK","VPST 4,5x 200",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 45kg, průměr svazku 50mm, rozměr 4,5x201x0,3mm","100ks",22.453061966739778,{"$f":"F2696*(1-Elteq!$F$9)","v":22.453061966739778},"8591735019525"]
["TECHNIK","VPST 4,5x 200/316",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 45kg, průměr svazku 50mm, rozměr 4,5x201x0,3mm","100ks",27.092124356562046,{"$f":"F2697*(1-Elteq!$F$9)","v":27.092124356562046},"8591735052140"]
["TECHNIK","VPST 4,5x 265",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 45kg, průměr svazku 65mm, rozměr 4,5x265x0,3mm","100ks",25.236499400633139,{"$f":"F2698*(1-Elteq!$F$9)","v":25.236499400633139},"8591735046477"]
["TECHNIK","VPST 4,5x 300",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 45kg, průměr svazku 80mm, rozměr 4,5x300x0,3mm","100ks",25.9787493830047,{"$f":"F2699*(1-Elteq!$F$9)","v":25.9787493830047},"8591735046507"]
["TECHNIK","VPST 4,5x 360",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 45kg, průměr svazku 95mm, rozměr 4,5x362x0,3mm","100ks",26.535436869783375,{"$f":"F2700*(1-Elteq!$F$9)","v":26.535436869783375},"8591735019532"]
["TECHNIK","VPST 4,5x 520",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 45kg, průměr svazku 152mm, rozměr 4,5x521x0,3mm","100ks",37.29806161417104,{"$f":"F2701*(1-Elteq!$F$9)","v":37.29806161417104},"8591735019563"]
["TECHNIK","VPST 4,5x 680",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 45kg, průměr svazku 195mm, rozměr 4,5x679x0,3mm","100ks",63.833498483954408,{"$f":"F2702*(1-Elteq!$F$9)","v":63.833498483954408},"8591735023003"]
["TECHNIK","VPST 4,5x 840",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 45kg, průměr svazku 250mm, rozměr 4,5x838x0,3mm","100ks",66.431373422254879,{"$f":"F2703*(1-Elteq!$F$9)","v":66.431373422254879},"8591735023010"]
["TECHNIK","VPST 4,5x1060",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 45kg, průměr svazku 318mm, rozměr 4,5x1060x0,3mm","100ks",79.977435600535898,{"$f":"F2704*(1-Elteq!$F$9)","v":79.977435600535898},"8591735023027"]
["TECHNIK","VPST 4,5x1190",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 45kg, průměr svazku 360mm, rozměr 4,5x1194x0,3mm","100ks",104.2861225232046,{"$f":"F2705*(1-Elteq!$F$9)","v":104.2861225232046},"8591735046521"]
["TECHNIK","VPST 6,3x 150 NL",null,"Vázací páska nerezová rozebíratelná 6,35x152mm, nosnost 45kg, svazek 38mm potažená nylonem AE111","100ks",87.771060415437319,{"$f":"F2706*(1-Elteq!$F$9)","v":87.771060415437319},"8591735052218"]
["TECHNIK","VPST 6,3x 230 NL",null,"Vázací páska nerezová rozebíratelná 6,35x229mm, nosnost 45kg, svazek 63mm potažená nylonem AE112","100ks",98.719247655417874,{"$f":"F2707*(1-Elteq!$F$9)","v":98.719247655417874},"8591735052201"]
["TECHNIK","VPST 6,3x 300 NL",null,"Vázací páska nerezová rozebíratelná 6,35x305mm, nosnost 45kg, svazek 86mm potažená nylonem AE113","100ks",111.15193486014155,{"$f":"F2708*(1-Elteq!$F$9)","v":111.15193486014155},"8591735052195"]
["TECHNIK","VPST 8x 152",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 113kg, max. svazek 35mm, rozměr 8,0x152x0,3mm","100ks",27.83437433893361,{"$f":"F2709*(1-Elteq!$F$9)","v":27.83437433893361},"8591735023034"]
["TECHNIK","VPST 8x 152 EX",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 113kg, max. svazek 35mm, potažená epoxydem","100ks",71.07043581207715,{"$f":"F2710*(1-Elteq!$F$9)","v":71.07043581207715},"8591735046989"]
["TECHNIK","VPST 8x 200",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 113kg, max. svazek 50mm, rozměr 8,0x201x0,3mm","100ks",28.947749312490952,{"$f":"F2711*(1-Elteq!$F$9)","v":28.947749312490952},"8591735023041"]
["TECHNIK","VPST 8x 200 EX",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 113kg, max. svazek 50mm, potažená epoxydem","100ks",78.307373140199886,{"$f":"F2712*(1-Elteq!$F$9)","v":78.307373140199886},"8591735046941"]
["TECHNIK","VPST 8x 200 NL",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 113kg, max. svazek 50mm, potažená nylonem MLTC2H","100ks",165.15062107767275,{"$f":"F2713*(1-Elteq!$F$9)","v":165.15062107767275},"8591735052768"]
["TECHNIK","VPST 8x 265",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 113kg, max. svazek 65mm, rozměr 8,0x266x0,3mm","100ks",30.061124286048297,{"$f":"F2714*(1-Elteq!$F$9)","v":30.061124286048297},"8591735046484"]
["TECHNIK","VPST 8x 265 EX",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 113kg, max. svazek 65mm, potažená epoxydem","100ks",90.183372858144892,{"$f":"F2715*(1-Elteq!$F$9)","v":90.183372858144892},"8591735046927"]
["TECHNIK","VPST 8x 300",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 113kg, max. svazek 80mm, rozměr 8,0x300x0,3mm","100ks",31.731186746384314,{"$f":"F2716*(1-Elteq!$F$9)","v":31.731186746384314},"8591735046514"]
["TECHNIK","VPST 8x 300 EX",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 113kg, max. svazek 80mm, potažená epoxydem","100ks",97.420310186267628,{"$f":"F2717*(1-Elteq!$F$9)","v":97.420310186267628},"8591735046910"]
["TECHNIK","VPST 8x 300 PR",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 113kg, max. svazek 80mm, potažená polyesterem","100ks",351.82649164412084,{"$f":"F2718*(1-Elteq!$F$9)","v":351.82649164412084},"8591735048501"]
["TECHNIK","VPST 8x 360",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 113kg, max. svazek 95mm, rozměr 8,0x362x0,3mm","100ks",33.77237419790611,{"$f":"F2719*(1-Elteq!$F$9)","v":33.77237419790611},"8591735023058"]
["TECHNIK","VPST 8x 360 EX",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 113kg, max.svazek 95mm, potažená epoxydem KE0448","100ks",102.61606006286857,{"$f":"F2720*(1-Elteq!$F$9)","v":102.61606006286857},"8591735046958"]
["TECHNIK","VPST 8x 360 NL",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 113kg, max. svazek 95mm, potažená nylonem MLTC4H","100ks",226.38624462332669,{"$f":"F2721*(1-Elteq!$F$9)","v":226.38624462332669},"8591735048518"]
["TECHNIK","VPST 8x 520",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 113kg, max. svazek 152mm, rozměr 8,0x521x0,3mm","100ks",46.019498907036898,{"$f":"F2722*(1-Elteq!$F$9)","v":46.019498907036898},"8591735023065"]
["TECHNIK","VPST 8x 520 EX",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 113kg, max.svazek 152mm, potažená epoxydem KE0458","100ks",125.25468452520124,{"$f":"F2723*(1-Elteq!$F$9)","v":125.25468452520124},"8591735046934"]
["TECHNIK","VPST 8x 520 NL",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 113kg, max. svazek 152mm, potažená nylonem MLTC6H","100ks",279.08599337170767,{"$f":"F2724*(1-Elteq!$F$9)","v":279.08599337170767},"8591735054984"]
["TECHNIK","VPST 8x 680",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 113kg, max. svazek 203mm, rozměr 8,0x679x0,3mm","100ks",95.193560239152944,{"$f":"F2725*(1-Elteq!$F$9)","v":95.193560239152944},"8591735023072"]
["TECHNIK","VPST 8x 680 EX",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 113kg, max.svazek 203mm, potažená epoxydem KE0468","100ks",168.49074599834478,{"$f":"F2726*(1-Elteq!$F$9)","v":168.49074599834478},"8591735046965"]
["TECHNIK","VPST 8x 840",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 113kg, max. svazek 254mm, rozměr 8,0x838x0,3mm","100ks",103.54387254083302,{"$f":"F2727*(1-Elteq!$F$9)","v":103.54387254083302},"8591735023089"]
["TECHNIK","VPST 8x 840 EX",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 113kg, max.svazek 254mm, potažená epoxydem KE0478","100ks",190.57268297389879,{"$f":"F2728*(1-Elteq!$F$9)","v":190.57268297389879},"8591735046972"]
["TECHNIK","VPST 8x1060",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 113kg, max.svazek 318mm, rozměr 8,0x1060x0,3mm","100ks",133.41943433128844,{"$f":"F2729*(1-Elteq!$F$9)","v":133.41943433128844},"8591735023096"]
["TECHNIK","VPST 8x1060 EX",null,"Vázací páska nerezová s kuličkovým zámkem, nosnost 113kg, max. svazek 318mm, potažená epoxydem","100ks",208.57224504640919,{"$f":"F2730*(1-Elteq!$F$9)","v":208.57224504640919},"8591735046996"]
["TECHNIK","VPP  1,7x70",null,"Vázací páska přírodní, nosnost 3kg, průměr svazku 11mm, rozměr 1,7x70mm","100ks",0.70513748325298475,{"$f":"F2731*(1-Elteq!$F$9)","v":0.70513748325298475},"8591735037659"]
["TECHNIK","VPP  1,9x100",null,"Vázací páska přírodní, nosnost 5kg, průměr svazku 22mm, rozměr 1,95x103mm","100ks",0.81647498060871926,{"$f":"F2732*(1-Elteq!$F$9)","v":0.81647498060871926},"8591735051815"]
["TECHNIK","VPP  2,4x60",null,"Vázací páska přírodní, nosnost 8kg, průměr svazku 11mm, rozměr 2,4x60mm","100ks",0.42679373986364866,{"$f":"F2733*(1-Elteq!$F$9)","v":0.42679373986364866},"8591735022860"]
["TECHNIK","VPP  2,4x80",null,"Vázací páska přírodní, nosnost 8kg, průměr svazku 15mm, rozměr 2,4x80mm","100ks",0.46390623898222683,{"$f":"F2734*(1-Elteq!$F$9)","v":0.46390623898222683},"8591735004729"]
["TECHNIK","VPP  2,5x100",null,"Vázací páska přírodní, nosnost 8kg, průměr svazku 22mm, rozměr 2,5x100mm","100ks",0.37112499118578146,{"$f":"F2735*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735002039"]
["TECHNIK","VPP  2,5x100/1000",null,"Vázací páska přírodní, nosnost 8kg, průměr svazku 22mm, rozměr 2,5x100mm (po 1000ks)","1000ks",3.7112499118578146,{"$f":"F2736*(1-Elteq!$F$9)","v":3.7112499118578146},"8591735037864"]
["TECHNIK","VPP  2,5x120",null,"Vázací páska přírodní, nosnost 8kg, průměr svazku 30mm, rozměr 2,5x120mm","100ks",0.59379998589725036,{"$f":"F2737*(1-Elteq!$F$9)","v":0.59379998589725036},"8591735008390"]
["TECHNIK","VPP  2,5x140",null,"Vázací páska přírodní, nosnost 8kg, průměr svazku 33mm, rozměr 2,5x140mm","100ks",0.64946873457511756,{"$f":"F2738*(1-Elteq!$F$9)","v":0.64946873457511756},"8591735004736"]
["TECHNIK","VPP  2,5x160",null,"Vázací páska přírodní, nosnost 8kg, průměr svazku 40mm, rozměr 2,5x160mm","100ks",0.77936248149014109,{"$f":"F2739*(1-Elteq!$F$9)","v":0.77936248149014109},"8591735004743"]
["TECHNIK","VPP  2,5x200",null,"Vázací páska přírodní, nosnost 8kg, průměr svazku 53mm, rozměr 2,5x200mm","100ks",0.83503123016800829,{"$f":"F2740*(1-Elteq!$F$9)","v":0.83503123016800829},"8591735004750"]
["TECHNIK","VPP  3,6x140",null,"Vázací páska přírodní, nosnost 18kg, průměr svazku 33mm, rozměr 3,6x140mm","100ks",0.70513748325298475,{"$f":"F2741*(1-Elteq!$F$9)","v":0.70513748325298475},"8591735004767"]
["TECHNIK","VPP  3,6x150",null,"Vázací páska přírodní, nosnost 18kg, průměr svazku 35mm, rozměr 3,6x150mm","100ks",1.0577062248794771,{"$f":"F2742*(1-Elteq!$F$9)","v":1.0577062248794771},"8591735011147"]
["TECHNIK","VPP  3,6x180",null,"Vázací páska přírodní, nosnost 18kg, průměr svazku 47mm, rozměr 3,6x180mm","100ks",1.4288312160652585,{"$f":"F2743*(1-Elteq!$F$9)","v":1.4288312160652585},"8591735021139"]
["TECHNIK","VPP  3,6x200",null,"Vázací páska přírodní, nosnost 18kg, průměr svazku 53mm, rozměr 3,6x200mm","100ks",1.4473874656245478,{"$f":"F2744*(1-Elteq!$F$9)","v":1.4473874656245478},"8591735004774"]
["TECHNIK","VPP  3,6x250",null,"Vázací páska přírodní, nosnost 18kg, průměr svazku 65mm, rozměr 3,6x250mm","100ks",1.8185124568103292,{"$f":"F2745*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735019129"]
["TECHNIK","VPP  3,6x300",null,"Vázací páska přírodní, nosnost 18kg, průměr svazku 76mm, rozměr 3,6x292mm","100ks",1.8370687063696183,{"$f":"F2746*(1-Elteq!$F$9)","v":1.8370687063696183},"8591735004781"]
["TECHNIK","VPP  3,6x370",null,"Vázací páska přírodní, nosnost 18kg, průměr svazku 102mm, rozměr 3,6x370mm","100ks",2.6535436869783373,{"$f":"F2747*(1-Elteq!$F$9)","v":2.6535436869783373},"8591735004798"]
["TECHNIK","VPP  4,8x120",null,"Vázací páska přírodní, nosnost 22kg, průměr svazku 28mm, rozměr 4,8x120mm","100ks",1.4102749665059695,{"$f":"F2748*(1-Elteq!$F$9)","v":1.4102749665059695},"8591735022877"]
["TECHNIK","VPP  4,8x160",null,"Vázací páska přírodní, nosnost 22kg, průměr svazku 38mm, rozměr 4,8x160mm","100ks",1.4473874656245478,{"$f":"F2749*(1-Elteq!$F$9)","v":1.4473874656245478},"8591735010669"]
["TECHNIK","VPP  4,8x188",null,"Vázací páska přírodní, nosnost 22kg, průměr svazku 46mm, rozměr 4,8x188mm","100ks",1.4659437151838368,{"$f":"F2750*(1-Elteq!$F$9)","v":1.4659437151838368},"8591735010645"]
["TECHNIK","VPP  4,8x200",null,"Vázací páska přírodní, nosnost 22kg, průměr svazku 50mm, rozměr 4,8x200mm","100ks",1.4844999647431258,{"$f":"F2751*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735004804"]
["TECHNIK","VPP  4,8x250",null,"Vázací páska přírodní, nosnost 22kg, průměr svazku 60mm, rozměr 4,8x250mm","100ks",2.1525249488775327,{"$f":"F2752*(1-Elteq!$F$9)","v":2.1525249488775327},"8591735004811"]
["TECHNIK","VPP  4,8x280",null,"Vázací páska přírodní, nosnost 22kg, průměr svazku 70mm, rozměr 4,8x280mm","100ks",2.2453061966739778,{"$f":"F2753*(1-Elteq!$F$9)","v":2.2453061966739778},"8591735004828"]
["TECHNIK","VPP  4,8x300",null,"Vázací páska přírodní, nosnost 22kg, průměr svazku 76mm, rozměr 4,8x300mm","100ks",2.2824186957925559,{"$f":"F2754*(1-Elteq!$F$9)","v":2.2824186957925559},"8591735004835"]
["TECHNIK","VPP  4,8x370",null,"Vázací páska přírodní, nosnost 22kg, průměr svazku 102mm, rozměr 4,8x368mm","100ks",2.5422061896226031,{"$f":"F2755*(1-Elteq!$F$9)","v":2.5422061896226031},"8591735004842"]
["TECHNIK","VPP  4,8x430",null,"Vázací páska přírodní, nosnost 22kg, průměr svazku 110mm, rozměr 4,8x430mm","100ks",4.9359623827708932,{"$f":"F2756*(1-Elteq!$F$9)","v":4.9359623827708932},"8591735004859"]
["TECHNIK","VPP  4,8x530",null,"Vázací páska přírodní, nosnost 22kg, průměr svazku 140mm, rozměr 4,8x530mm","100ks",7.7565123157828326,{"$f":"F2757*(1-Elteq!$F$9)","v":7.7565123157828326},"8591735009786"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"VPP  4,8x680",null,"Vázací páska přírodní, nosnost 22kg, průměr svazku 205mm, rozměr 4,8x685mm","100ks",14.39964965800832,{"$f":"F2758*(1-Elteq!$F$9)","v":14.39964965800832},"8591735019433"]
["TECHNIK","VPP  4,8x830",null,"Vázací páska přírodní, nosnost 22kg, průměr svazku 250mm, rozměr 4,8x830mm","100ks",15.80992462451429,{"$f":"F2759*(1-Elteq!$F$9)","v":15.80992462451429},"8591735019440"]
["TECHNIK","VPP  7,6x150",null,"Vázací páska přírodní, nosnost 54kg, průměr svazku 33mm, rozměr 7,6x150mm","100ks",3.7112499118578146,{"$f":"F2760*(1-Elteq!$F$9)","v":3.7112499118578146},"8591735019457"]
["TECHNIK","VPP  7,6x200",null,"Vázací páska přírodní, nosnost 54kg, průměr svazku 50mm, rozměr 7,6x200mm","100ks",4.3421623968736434,{"$f":"F2761*(1-Elteq!$F$9)","v":4.3421623968736434},"8591735004866"]
["TECHNIK","VPP  7,6x240",null,"Vázací páska přírodní, nosnost 54kg, průměr svazku 60mm, rozměr 7,6x240mm","100ks",4.8988498836523151,{"$f":"F2762*(1-Elteq!$F$9)","v":4.8988498836523151},"8591735016265"]
["TECHNIK","VPP  7,6x300",null,"Vázací páska přírodní, nosnost 54kg, průměr svazku 76mm, rozměr 7,6x292mm","100ks",4.9730748818894712,{"$f":"F2763*(1-Elteq!$F$9)","v":4.9730748818894712},"8591735004873"]
["TECHNIK","VPP  7,6x370",null,"Vázací páska přírodní, nosnost 54kg, průměr svazku 102mm, rozměr 7,6x368mm","100ks",5.1957498766009405,{"$f":"F2764*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735004880"]
["TECHNIK","VPP  7,8x450",null,"Vázací páska přírodní, nosnost 54kg, průměr svazku 125mm, rozměr 7,8x450mm","100ks",9.0925622840516453,{"$f":"F2765*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735004897"]
["TECHNIK","VPP  7,8x550",null,"Vázací páska přírodní, nosnost 54kg, průměr svazku 160mm, rozměr 7,8x550mm","100ks",10.354387254083303,{"$f":"F2766*(1-Elteq!$F$9)","v":10.354387254083303},"8591735004903"]
["TECHNIK","VPP  7,8x750",null,"Vázací páska přírodní, nosnost 54kg, průměr svazku 216mm, rozměr 7,8x750mm","100ks",16.774849601597321,{"$f":"F2767*(1-Elteq!$F$9)","v":16.774849601597321},"8591735005184"]
["TECHNIK","VPP  9,0x 430",null,"Vázací páska přírodní, nosnost 77kg, průměr svazku 125mm, rozměr 9x430mm","100ks",12.61824970031657,{"$f":"F2768*(1-Elteq!$F$9)","v":12.61824970031657},"8591735004927"]
["TECHNIK","VPP  9,0x 530",null,"Vázací páska přírodní, nosnost 77kg, průměr svazku 140mm, rozměr 9x530mm","100ks",15.216124638617039,{"$f":"F2769*(1-Elteq!$F$9)","v":15.216124638617039},"8591735004934"]
["TECHNIK","VPP  9,0x 780",null,"Vázací páska přírodní, nosnost 77kg, průměr svazku 228mm, rozměr 9x780mm","100ks",17.81399957691751,{"$f":"F2770*(1-Elteq!$F$9)","v":17.81399957691751},"8591735004941"]
["TECHNIK","VPP  9,0x1020",null,"Vázací páska přírodní, nosnost 77kg, průměr svazku 295mm, rozměr 9x1020mm","100ks",32.287874233162988,{"$f":"F2771*(1-Elteq!$F$9)","v":32.287874233162988},"8591735007317"]
["TECHNIK","VPP  9,0x1220",null,"Vázací páska přírodní, nosnost 77kg, průměr svazku 352mm, rozměr 9x1220mm","100ks",46.019498907036898,{"$f":"F2772*(1-Elteq!$F$9)","v":46.019498907036898},"8591735004958"]
["TECHNIK","VPP  9,0x1530",null,"Vázací páska přírodní, nosnost 77kg, průměr svazku 455mm, rozměr 9x1530mm","100ks",64.761310961918866,{"$f":"F2773*(1-Elteq!$F$9)","v":64.761310961918866},"8591735019464"]
["TECHNIK","VPP 13x 230",null,"Vázací páska přírodní, nosnost 110kg, průměr svazku 50mm, rozměr 13x230mm","100ks",13.100712188858086,{"$f":"F2774*(1-Elteq!$F$9)","v":13.100712188858086},"8591735005245"]
["TECHNIK","VPP 13x 380",null,"Vázací páska přírodní, nosnost 110kg, průměr svazku 96mm, rozměr 13x380mm","100ks",17.81399957691751,{"$f":"F2775*(1-Elteq!$F$9)","v":17.81399957691751},"8591735019471"]
["TECHNIK","VPP 13x 480",null,"Vázací páska přírodní, nosnost 110kg, průměr svazku 121mm, rozměr 13x480mm","100ks",18.185124568103291,{"$f":"F2776*(1-Elteq!$F$9)","v":18.185124568103291},"8591735007188"]
["TECHNIK","VPP 13x 580",null,"Vázací páska přírodní, nosnost 110kg, průměr svazku 140mm, rozměr 13x580mm","100ks",24.494249418261575,{"$f":"F2777*(1-Elteq!$F$9)","v":24.494249418261575},"8591735005252"]
["TECHNIK","VPP 13x 730",null,"Vázací páska přírodní, nosnost 110kg, průměr svazku 200mm, rozměr 13x730mm","100ks",24.679811913854468,{"$f":"F2778*(1-Elteq!$F$9)","v":24.679811913854468},"8591735005269"]
["TECHNIK","VPP 13x 830",null,"Vázací páska přírodní, nosnost 110kg, průměr svazku 219mm, rozměr 13x830mm","100ks",41.937124003993304,{"$f":"F2779*(1-Elteq!$F$9)","v":41.937124003993304},"8591735019488"]
["TECHNIK","VPP 13x1000",null,"Vázací páska přírodní, nosnost 110kg, průměr svazku 300mm, rozměr 13x1000mm","100ks",42.308248995179085,{"$f":"F2780*(1-Elteq!$F$9)","v":42.308248995179085},"8591735005276"]
["TECHNIK","VP RAPSTRAP černá",null,"Vázací páska vícenásobná - rozebíratelná, nosnost 12kg, prům. svazku 120mm, rozměr 10x300mm černá UV","24ks",2.1525249488775327,{"$f":"F2781*(1-Elteq!$F$9)","v":2.1525249488775327},"8591735042295"]
["TECHNIK","VP RAPSTRAP přírodní",null,"Vázací páska vícenásobná - rozebíratelná, nosnost 12kg, prům. svazku 120mm, rozměr 10x300mm přírodní","24ks",2.1525249488775327,{"$f":"F2782*(1-Elteq!$F$9)","v":2.1525249488775327},"8591735051983"]
["TECHNIK","VP RAPSTRAP rudá",null,"Vázací páska vícenásobná - rozebíratelná, nosnost 12kg, prům. svazku 120mm, rozměr 10x300mm rudá","24ks",3.0432249277234078,{"$f":"F2783*(1-Elteq!$F$9)","v":3.0432249277234078},"8591735052003"]
["TECHNIK","VP RAPSTRAP zelená",null,"Vázací páska vícenásobná - rozebíratelná, nosnost 12kg, prům. svazku 120mm, rozměr 10x300mm zelená","24ks",3.0432249277234078,{"$f":"F2784*(1-Elteq!$F$9)","v":3.0432249277234078},"8591735051990"]
["TECHNIK","VPCRO 3,6x100",null,"Vázací páska černá rozebíratelná 3,6x100mm","100ks",5.3813123721938307,{"$f":"F2785*(1-Elteq!$F$9)","v":5.3813123721938307},"8591735022891"]
["TECHNIK","VPCRO 4,8x150",null,"Vázací páska černá rozebíratelná 4,8x150mm","100ks",5.7524373633796122,{"$f":"F2786*(1-Elteq!$F$9)","v":5.7524373633796122},"8591735022907"]
["TECHNIK","VPCRO 4,8x200",null,"Vázací páska černá rozebíratelná 4,8x200mm","100ks",6.2720123510397068,{"$f":"F2787*(1-Elteq!$F$9)","v":6.2720123510397068},"8591735018962"]
["TECHNIK","VPCRO 4,8x250",null,"Vázací páska černá rozebíratelná 4,8x250mm","100ks",9.8348122664232083,{"$f":"F2788*(1-Elteq!$F$9)","v":9.8348122664232083},"8591735020064"]
["TECHNIK","VPCRO 4,8x300",null,"Vázací páska černá rozebíratelná 4,8x300mm","100ks",10.131712259371835,{"$f":"F2789*(1-Elteq!$F$9)","v":10.131712259371835},"8591735020071"]
["TECHNIK","VPCRO 4,8x370",null,"Vázací páska černá rozebíratelná 4,8x370mm","100ks",12.135787211775053,{"$f":"F2790*(1-Elteq!$F$9)","v":12.135787211775053},"8591735020088"]
["TECHNIK","VPCRO 7,6x120",null,"Vázací páska černá rozebíratelná 7,6x120mm","100ks",11.504874726759224,{"$f":"F2791*(1-Elteq!$F$9)","v":11.504874726759224},"8591735034344"]
["TECHNIK","VPCRO 7,6x150",null,"Vázací páska černá rozebíratelná 7,6x150mm","100ks",12.469799703842257,{"$f":"F2792*(1-Elteq!$F$9)","v":12.469799703842257},"8591735010607"]
["TECHNIK","VPCRO 7,6x200",null,"Vázací páska černá rozebíratelná 7,6x200mm","100ks",12.952262192383772,{"$f":"F2793*(1-Elteq!$F$9)","v":12.952262192383772},"8591735010614"]
["TECHNIK","VPCRO 7,6x250",null,"Vázací páska černá rozebíratelná 7,6x250mm","100ks",13.323387183569555,{"$f":"F2794*(1-Elteq!$F$9)","v":13.323387183569555},"8591735038069"]
["TECHNIK","VPCRO 7,6x300",null,"Vázací páska černá rozebíratelná 7,6x300mm","100ks",13.694512174755335,{"$f":"F2795*(1-Elteq!$F$9)","v":13.694512174755335},"8591735010621"]
["TECHNIK","VPCRO12,4x400",null,"Vázací páska černá rozebíratelná 12,4x400mm","100ks",34.625961677633413,{"$f":"F2796*(1-Elteq!$F$9)","v":34.625961677633413},"8591735050764"]
["TECHNIK","VPCRO12,4x500",null,"Vázací páska černá rozebíratelná 12,4x500mm","100ks",42.122686499586194,{"$f":"F2797*(1-Elteq!$F$9)","v":42.122686499586194},"8591735049300"]
["TECHNIK","VPRO 3,6x100",null,"Vázací páska přírodní rozebíratelná 3,6x100mm","100ks",5.3813123721938307,{"$f":"F2798*(1-Elteq!$F$9)","v":5.3813123721938307},"8591735009946"]
["TECHNIK","VPRO 4,8x150",null,"Vázací páska přírodní rozebíratelná 4,8x150mm","100ks",5.7524373633796122,{"$f":"F2799*(1-Elteq!$F$9)","v":5.7524373633796122},"8591735009953"]
["TECHNIK","VPRO 4,8x200",null,"Vázací páska přírodní rozebíratelná 4,8x200mm","100ks",6.2720123510397068,{"$f":"F2800*(1-Elteq!$F$9)","v":6.2720123510397068},"8591735009960"]
["TECHNIK","VPRO 4,8x250",null,"Vázací páska přírodní rozebíratelná 4,8x250mm","100ks",9.8348122664232083,{"$f":"F2801*(1-Elteq!$F$9)","v":9.8348122664232083},"8591735020095"]
["TECHNIK","VPRO 4,8x300",null,"Vázací páska přírodní rozebíratelná 4,8x300mm","100ks",10.131712259371835,{"$f":"F2802*(1-Elteq!$F$9)","v":10.131712259371835},"8591735009977"]
["TECHNIK","VPRO 4,8x370",null,"Vázací páska přírodní rozebíratelná 4,8x370mm","100ks",12.135787211775053,{"$f":"F2803*(1-Elteq!$F$9)","v":12.135787211775053},"8591735009984"]
["TECHNIK","VPRO 7,6x120",null,"Vázací páska přírodní rozebíratelná 7,6x120mm","100ks",11.504874726759224,{"$f":"F2804*(1-Elteq!$F$9)","v":11.504874726759224},"8591735034399"]
["TECHNIK","VPRO 7,6x150",null,"Vázací páska přírodní rozebíratelná 7,6x150mm","100ks",12.469799703842257,{"$f":"F2805*(1-Elteq!$F$9)","v":12.469799703842257},"8591735022914"]
["TECHNIK","VPRO 7,6x200",null,"Vázací páska přírodní rozebíratelná 7,6x200mm","100ks",12.952262192383772,{"$f":"F2806*(1-Elteq!$F$9)","v":12.952262192383772},"8591735022921"]
["TECHNIK","VPRO 7,6x300",null,"Vázací páska přírodní rozebíratelná 7,6x300mm","100ks",13.694512174755335,{"$f":"F2807*(1-Elteq!$F$9)","v":13.694512174755335},"8591735022938"]
["TECHNIK","VPRO12,4x400",null,"Vázací páska přírodní rozebíratelná 12,4x400mm","100ks",34.625961677633413,{"$f":"F2808*(1-Elteq!$F$9)","v":34.625961677633413},""]
["TECHNIK","VPRO12,4x500",null,"Vázací páska přírodní rozebíratelná 12,4x500mm","100ks",42.122686499586194,{"$f":"F2809*(1-Elteq!$F$9)","v":42.122686499586194},""]
["TECHNIK","VPCFE 2,4x 90",null,"Vázací páska černá s kovovým jazýčkem, nosnost 8kg, průměr svazku 16mm, rozměr 2,4x92mm TY23MX","1000ks",40.452624039250182,{"$f":"F2810*(1-Elteq!$F$9)","v":40.452624039250182},"8591735034504"]
["TECHNIK","VPCFE 2,4x200",null,"Vázací páska černá s kovovým jazýčkem, nosnost 8kg, průměr svazku 50mm, rozměr 2,4x200mm TY232MX","1000ks",65.132435953104647,{"$f":"F2811*(1-Elteq!$F$9)","v":65.132435953104647},"8591735034511"]
["TECHNIK","VPCFE 3,6x140",null,"Vázací páska černá s kovovým jazýčkem, nosnost 18kg, průměr svazku 29mm, rozměr 3,6x140mm TY24MX","1000ks",54.555373704309872,{"$f":"F2812*(1-Elteq!$F$9)","v":54.555373704309872},"8591735034528"]
["TECHNIK","VPCFE 3,6x200",null,"Vázací páska černá s kovovým jazýčkem, nosnost 18kg, průměr svazku 53mm, rozměr 3,6x200mm TY242MX","1000ks",91.111185336109344,{"$f":"F2813*(1-Elteq!$F$9)","v":91.111185336109344},"8591735034535"]
["TECHNIK","VPCFE 3,6x280",null,"Vázací páska černá s kovovým jazýčkem, nosnost 18kg, průměr svazku 76mm, rozměr 3,6x281mm TY26MX","1000ks",147.70774649194101,{"$f":"F2814*(1-Elteq!$F$9)","v":147.70774649194101},"8591735034542"]
["TECHNIK","VPCFE 3,6x370",null,"Vázací páska černá s kovovým jazýčkem, nosnost 18kg, průměr svazku 103mm, rozměr 3,6x368mm TY244MX","1000ks",275.56030595544274,{"$f":"F2815*(1-Elteq!$F$9)","v":275.56030595544274},"8591735034559"]
["TECHNIK","VPCFE 4,8x180",null,"Vázací páska černá s kovovým jazýčkem, nosnost 22kg, průměr svazku 45mm, rozměr 4,8x186mm TY25MX","1000ks",79.235185618164337,{"$f":"F2816*(1-Elteq!$F$9)","v":79.235185618164337},"8591735034566"]
["TECHNIK","VPCFE 4,8x290",null,"Vázací páska černá s kovovým jazýčkem, nosnost 22kg, průměr svazku 78mm, rozměr 4,8x293mm TY253MX","1000ks",210.24230750674519,{"$f":"F2817*(1-Elteq!$F$9)","v":210.24230750674519},"8591735034573"]
["TECHNIK","VPCFE 4,8x360",null,"Vázací páska černá s kovovým jazýčkem, nosnost 22kg, průměr svazku 102mm, rozměr 4,8x360mm TY28MX","1000ks",179.62449573391822,{"$f":"F2818*(1-Elteq!$F$9)","v":179.62449573391822},"8591735034580"]
["TECHNIK","VPCFE 7,6x222",null,"Vázací páska černá s kovovým jazýčkem, nosnost 50kg, průměr svazku 50mm, rozměr 7,6x222mm TY272MX","500ks",229.16968205722006,{"$f":"F2819*(1-Elteq!$F$9)","v":229.16968205722006},"8591735049584"]
["TECHNIK","VPCFE 7,6x340",null,"Vázací páska černá s kovovým jazýčkem, nosnost 50kg, průměr svazku 90mm, rozměr 7,6x340mm TY27MX","500ks",153.27462135972775,{"$f":"F2820*(1-Elteq!$F$9)","v":153.27462135972775},"8591735034597"]
["TECHNIK","VPCFE 7,6x760",null,"Vázací páska černá s kovovým jazýčkem, nosnost 50kg, průměr svazku 210mm, rozměr 7,6x760mm TY29MX","500ks",409.72199026910272,{"$f":"F2821*(1-Elteq!$F$9)","v":409.72199026910272},"8591735034603"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"VPPFE 2,4x 90",null,"Vázací páska přírodní s kovovým jazýčkem, nosnost 8kg, průměr svazku 16mm, rozměr 2,4x92mm TY23M","1000ks",34.514624180277679,{"$f":"F2822*(1-Elteq!$F$9)","v":34.514624180277679},"8591735034610"]
["TECHNIK","VPPFE 2,4x200",null,"Vázací páska přírodní s kovovým jazýčkem, nosnost 8kg, průměr svazku 50mm, rozměr 2,4x200mm TY232M","1000ks",68.101435882590891,{"$f":"F2823*(1-Elteq!$F$9)","v":68.101435882590891},"8591735034627"]
["TECHNIK","VPPFE 2,4x360",null,"Vázací páska přírodní s kovovým jazýčkem, nosnost 8kg, průměr svazku 102mm, rozměr 2,4x356mm BT4M-M","1000ks",171.08862093664524,{"$f":"F2824*(1-Elteq!$F$9)","v":171.08862093664524},"8591735054168"]
["TECHNIK","VPPFE 3,6x140",null,"Vázací páska přírodní s kovovým jazýčkem, nosnost 18kg, průměr svazku 29mm, rozměr 3,6x140mm TY24M","1000ks",50.101873810080498,{"$f":"F2825*(1-Elteq!$F$9)","v":50.101873810080498},"8591735034634"]
["TECHNIK","VPPFE 3,6x200",null,"Vázací páska přírodní s kovovým jazýčkem, nosnost 18kg, průměr svazku 53mm, rozměr 3,6x200mm TY242M","1000ks",71.627123298855821,{"$f":"F2826*(1-Elteq!$F$9)","v":71.627123298855821},"8591735034641"]
["TECHNIK","VPPFE 3,6x280",null,"Vázací páska přírodní s kovovým jazýčkem, nosnost 18kg, průměr svazku 76mm, rozměr 3,6x280mm TY26M","1000ks",86.100997955101292,{"$f":"F2827*(1-Elteq!$F$9)","v":86.100997955101292},"8591735034658"]
["TECHNIK","VPPFE 3,6x370",null,"Vázací páska přírodní s kovovým jazýčkem, nosnost 18kg, průměr svazku 103mm, rozměr 3,6x368mm TY244M","1000ks",233.62318195144942,{"$f":"F2828*(1-Elteq!$F$9)","v":233.62318195144942},"8591735034665"]
["TECHNIK","VPPFE 4,8x180",null,"Vázací páska přírodní s kovovým jazýčkem, nosnost 22kg, průměr svazku 45mm, rozměr 4,8x186mm TY25M","1000ks",69.029248360555357,{"$f":"F2829*(1-Elteq!$F$9)","v":69.029248360555357},"8591735034672"]
["TECHNIK","VPPFE 4,8x290",null,"Vázací páska přírodní s kovovým jazýčkem, nosnost 22kg, průměr svazku 78mm, rozměr 4,8x293mm TY253M","1000ks",229.35524455281293,{"$f":"F2830*(1-Elteq!$F$9)","v":229.35524455281293},"8591735034689"]
["TECHNIK","VPPFE 4,8x360",null,"Vázací páska přírodní s kovovým jazýčkem, nosnost 22kg, průměr svazku 102mm, rozměr 4,8x360mm TY28M","1000ks",150.3056214302415,{"$f":"F2831*(1-Elteq!$F$9)","v":150.3056214302415},"8591735034696"]
["TECHNIK","VPPFE 7,6x340",null,"Vázací páska přírodní s kovovým jazýčkem, nosnost 50kg, průměr svazku 90mm, rozměr 7,6x340mm TY27M","500ks",87.956622911030209,{"$f":"F2832*(1-Elteq!$F$9)","v":87.956622911030209},"8591735034702"]
["TECHNIK","VPPFE 7,6x760",null,"Vázací páska přírodní s kovovým jazýčkem, nosnost 50kg, průměr svazku 210mm, rozměr 7,6x760mm TY29M","500ks",407.86636531317384,{"$f":"F2833*(1-Elteq!$F$9)","v":407.86636531317384},"8591735034719"]
["TECHNIK","VPS  2,5x100",null,"Vázací páska jednoduchá 2,5x100mm se štítkem 25,4x8mm","100ks",2.3751999435890014,{"$f":"F2834*(1-Elteq!$F$9)","v":2.3751999435890014},"8591735005320"]
["TECHNIK","VPS  2,5x110",null,"Vázací páska jednoduchá 2,5x110mm se štítkem 20,4x9,1mm","100ks",2.4494249418261576,{"$f":"F2835*(1-Elteq!$F$9)","v":2.4494249418261576},"8591735005337"]
["TECHNIK","VPS  2,5x130",null,"Vázací páska jednoduchá 2,5x130mm se štítkem 28x20mm","100ks",6.6431373422254882,{"$f":"F2836*(1-Elteq!$F$9)","v":6.6431373422254882},"8591735029999"]
["TECHNIK","VPS  2,5x200",null,"Vázací páska jednoduchá 2,5x200mm se štítkem 25,4x8mm","100ks",6.5689123439883321,{"$f":"F2837*(1-Elteq!$F$9)","v":6.5689123439883321},"8591735005344"]
["TECHNIK","VPS  2,5x210",null,"Vázací páska jednoduchá 2,5x210mm se štítkem 20,4x9,1mm","100ks",6.9029248360555355,{"$f":"F2838*(1-Elteq!$F$9)","v":6.9029248360555355},"8591735005351"]
["TECHNIK","VPS  4,8x220",null,"Vázací páska jednoduchá 4,8x220mm se štítkem 13x28mm","100ks",7.1255998307670039,{"$f":"F2839*(1-Elteq!$F$9)","v":7.1255998307670039},"8591735005368"]
["TECHNIK","VPS  4,8x270",null,"Vázací páska jednoduchá 4,8x270mm se štítkem 13x28mm","100ks",10.948187239980554,{"$f":"F2840*(1-Elteq!$F$9)","v":10.948187239980554},"8591735021276"]
["TECHNIK","VPS  4,8x300",null,"Vázací páska jednoduchá 4,8x300mm se štítkem 13x54mm","100ks",12.284237208249367,{"$f":"F2841*(1-Elteq!$F$9)","v":12.284237208249367},"8591735005375"]
["TECHNIK","VPS  4,8x370",null,"Vázací páska jednoduchá 4,8x370mm se štítkem 13x54mm","100ks",13.583174677399601,{"$f":"F2842*(1-Elteq!$F$9)","v":13.583174677399601},"8591735032180"]
["TECHNIK","VPS3  4,8x220",null,"Vázací páska trojitá 4,8x220mm se štítkem 47x28mm","100ks",16.626399605123009,{"$f":"F2843*(1-Elteq!$F$9)","v":16.626399605123009},"8591735033729"]
["TECHNIK","VPC+ 2,5x100",null,"Vázací páska termorezistentní, do 110°C dlouhodobě / do 145°C krátkodobě, černá","1000ks",5.3813123721938307,{"$f":"F2844*(1-Elteq!$F$9)","v":5.3813123721938307},"8591735022945"]
["TECHNIK","VPC+ 2,5x160",null,"Vázací páska termorezistentní, do 110°C dlouhodobě / do 145°C krátkodobě, černá","1000ks",12.061562213537897,{"$f":"F2845*(1-Elteq!$F$9)","v":12.061562213537897},"8591735022952"]
["TECHNIK","VPC+ 2,5x200",null,"Vázací páska termorezistentní, do 110°C dlouhodobě / do 145°C krátkodobě, černá","1000ks",12.469799703842257,{"$f":"F2846*(1-Elteq!$F$9)","v":12.469799703842257},"8591735029425"]
["TECHNIK","VPC+ 3,6x140",null,"Vázací páska termorezistentní, do 110°C dlouhodobě / do 145°C krátkodobě, černá","1000ks",11.133749735573444,{"$f":"F2847*(1-Elteq!$F$9)","v":11.133749735573444},"8591735022969"]
["TECHNIK","VPC+ 3,6x200",null,"Vázací páska termorezistentní, do 110°C dlouhodobě / do 145°C krátkodobě, černá","1000ks",20.782999506403762,{"$f":"F2848*(1-Elteq!$F$9)","v":20.782999506403762},"8591735029432"]
["TECHNIK","VPC+ 3,6x250",null,"Vázací páska termorezistentní, do 110°C dlouhodobě / do 145°C krátkodobě, černá","1000ks",35.25687416264924,{"$f":"F2849*(1-Elteq!$F$9)","v":35.25687416264924},"8591735029449"]
["TECHNIK","VPC+ 3,6x370",null,"Vázací páska termorezistentní, do 110°C dlouhodobě / do 145°C krátkodobě, černá","1000ks",36.741374127392362,{"$f":"F2850*(1-Elteq!$F$9)","v":36.741374127392362},"8591735029456"]
["TECHNIK","VPC+ 4,8x200",null,"Vázací páska termorezistentní, do 110°C dlouhodobě / do 145°C krátkodobě, černá","1000ks",16.329499612174384,{"$f":"F2851*(1-Elteq!$F$9)","v":16.329499612174384},"8591735022976"]
["TECHNIK","VPC+ 4,8x300",null,"Vázací páska termorezistentní, do 110°C dlouhodobě / do 145°C krátkodobě, černá","1000ks",26.535436869783375,{"$f":"F2852*(1-Elteq!$F$9)","v":26.535436869783375},"8591735033736"]
["TECHNIK","VPC+ 4,8x370",null,"Vázací páska termorezistentní, do 110°C dlouhodobě / do 145°C krátkodobě, černá (po 100ks)","1000ks",39.710374056878614,{"$f":"F2853*(1-Elteq!$F$9)","v":39.710374056878614},"8591735029418"]
["TECHNIK","VPC+ 4,8x430",null,"Vázací páska termorezistentní, do 110°C dlouhodobě / do 145°C krátkodobě, černá","100ks",10.762624744387661,{"$f":"F2854*(1-Elteq!$F$9)","v":10.762624744387661},"8591735029463"]
["TECHNIK","VPC+ 4,8x530",null,"Vázací páska termorezistentní, do 110°C dlouhodobě / do 145°C krátkodobě, černá","100ks",15.030562143024149,{"$f":"F2855*(1-Elteq!$F$9)","v":15.030562143024149},"8591735029470"]
["TECHNIK","VPC+ 7,6x370",null,"Vázací páska termorezistentní, do 110°C dlouhodobě / do 145°C krátkodobě, černá","100ks",6.3091248501582848,{"$f":"F2856*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735022983"]
["TECHNIK","VPC+ 9,0x780",null,"Vázací páska termorezistentní, do 110°C dlouhodobě / do 145°C krátkodobě, černá","100ks",27.871486838052189,{"$f":"F2857*(1-Elteq!$F$9)","v":27.871486838052189},"8591735022990"]
["TECHNIK","VPM+ 2,5x100",null,"Vázací páska termorezistentní, do 170°C dlouhodobě, barva modrá TEFZEL, rozměr 2,5x102mm","1000ks",522.5439875895803,{"$f":"F2858*(1-Elteq!$F$9)","v":522.5439875895803},"8591735046699"]
["TECHNIK","VPM+ 3,6x200",null,"Vázací páska termorezistentní, do 170°C dlouhodobě, barva modrá TEFZEL, rozměr 3,4x203mm","1000ks",673.59185900219336,{"$f":"F2859*(1-Elteq!$F$9)","v":673.59185900219336},"8591735046705"]
["TECHNIK","VPM+ 4,6x200",null,"Vázací páska termorezistentní, do 170°C dlouhodobě, barva modrá ETFE, rozměr 4,6x201mm (MOQ 200ks)","100ks",142.88312160652586,{"$f":"F2860*(1-Elteq!$F$9)","v":142.88312160652586},"8591735055080"]
["TECHNIK","VPM+ 4,8x190",null,"Vázací páska termorezistentní, do 170°C dlouhodobě, barva modrá TEFZEL, rozměr 4,8x188mm","1000ks",1200.9604714771888,{"$f":"F2861*(1-Elteq!$F$9)","v":1200.9604714771888},"8591735046712"]
["TECHNIK","VPM+ 4,8x300",null,"Vázací páska termorezistentní, do 170°C dlouhodobě, barva modrá TEFZEL, rozměr 4,8x295mm","1000ks",1789.5647074978383,{"$f":"F2862*(1-Elteq!$F$9)","v":1789.5647074978383},"8591735046729"]
["TECHNIK","VPM+ 4,8x370",null,"Vázací páska termorezistentní, do 170°C dlouhodobě, barva modrá TEFZEL, rozměr 4,8x371mm","1000ks",2413.7969426723225,{"$f":"F2863*(1-Elteq!$F$9)","v":2413.7969426723225},"8591735046736"]
["TECHNIK","VPR+ 2,5x100",null,"Vázací páska termorezistentní, do 130°C dlouhodobě / do 160°C krátkodobě, rubínová","100ks",0.66802498413440659,{"$f":"F2864*(1-Elteq!$F$9)","v":0.66802498413440659},"8591735029739"]
["TECHNIK","VPR+ 2,5x140",null,"Vázací páska termorezistentní, do 130°C dlouhodobě / do 160°C krátkodobě, rubínová","100ks",1.1875999717945007,{"$f":"F2865*(1-Elteq!$F$9)","v":1.1875999717945007},"8591735029760"]
["TECHNIK","VPR+ 2,5x160",null,"Vázací páska termorezistentní, do 130°C dlouhodobě / do 160°C krátkodobě, rubínová","100ks",1.5958374620988602,{"$f":"F2866*(1-Elteq!$F$9)","v":1.5958374620988602},"8591735029777"]
["TECHNIK","VPR+ 3,6x140",null,"Vázací páska termorezistentní, do 130°C dlouhodobě / do 160°C krátkodobě, rubínová","100ks",1.7071749594545946,{"$f":"F2867*(1-Elteq!$F$9)","v":1.7071749594545946},"8591735029746"]
["TECHNIK","VPR+ 3,6x200",null,"Vázací páska termorezistentní, do 130°C dlouhodobě / do 160°C krátkodobě, rubínová","100ks",2.5236499400633141,{"$f":"F2868*(1-Elteq!$F$9)","v":2.5236499400633141},"8591735029753"]
["TECHNIK","VPR+ 3,6x300",null,"Vázací páska termorezistentní, do 130°C dlouhodobě / do 160°C krátkodobě, rubínová","100ks",3.6370249136206585,{"$f":"F2869*(1-Elteq!$F$9)","v":3.6370249136206585},"8591735029784"]
["TECHNIK","VPR+ 3,6x360",null,"Vázací páska termorezistentní, do 130°C dlouhodobě / do 160°C krátkodobě, rubínová","100ks",5.3441998730752527,{"$f":"F2870*(1-Elteq!$F$9)","v":5.3441998730752527},"8591735029791"]
["TECHNIK","VPR+ 4,8x200",null,"Vázací páska termorezistentní, do 130°C dlouhodobě / do 160°C krátkodobě, rubínová","100ks",3.0061124286048297,{"$f":"F2871*(1-Elteq!$F$9)","v":3.0061124286048297},"8591735029807"]
["TECHNIK","VPR+ 4,8x250",null,"Vázací páska termorezistentní, do 130°C dlouhodobě / do 160°C krátkodobě, rubínová","100ks",3.8968124074507053,{"$f":"F2872*(1-Elteq!$F$9)","v":3.8968124074507053},"8591735029814"]
["TECHNIK","VPR+ 4,8x290",null,"Vázací páska termorezistentní, do 130°C dlouhodobě / do 160°C krátkodobě, rubínová","100ks",5.0101873810080493,{"$f":"F2873*(1-Elteq!$F$9)","v":5.0101873810080493},"8591735029821"]
["TECHNIK","VPR+ 4,8x360",null,"Vázací páska termorezistentní, do 130°C dlouhodobě / do 160°C krátkodobě, rubínová","100ks",6.0122248572096595,{"$f":"F2874*(1-Elteq!$F$9)","v":6.0122248572096595},"8591735029838"]
["TECHNIK","VPR+ 4,8x430",null,"Vázací páska termorezistentní, do 130°C dlouhodobě / do 160°C krátkodobě, rubínová","100ks",9.5750247725931619,{"$f":"F2875*(1-Elteq!$F$9)","v":9.5750247725931619},"8591735029845"]
["TECHNIK","VPR+ 4,8x530",null,"Vázací páska termorezistentní, do 130°C dlouhodobě / do 160°C krátkodobě, rubínová","100ks",13.434724680925289,{"$f":"F2876*(1-Elteq!$F$9)","v":13.434724680925289},"8591735029852"]
["TECHNIK","VPR+ 7,6x250",null,"Vázací páska termorezistentní, do 130°C dlouhodobě / do 160°C krátkodobě, rubínová","100ks",8.3503123016800824,{"$f":"F2877*(1-Elteq!$F$9)","v":8.3503123016800824},"8591735032272"]
["TECHNIK","VPR+ 7,6x360",null,"Vázací páska termorezistentní, do 130°C dlouhodobě / do 160°C krátkodobě, rubínová","100ks",10.799737243506241,{"$f":"F2878*(1-Elteq!$F$9)","v":10.799737243506241},"8591735032289"]
["TECHNIK","EDDING 140 S černá",null,"Permanentní pero s kulatým hrotem 0,3mm / barva černá","1ks",1.4844999647431258,{"$f":"F2879*(1-Elteq!$F$9)","v":1.4844999647431258},"4004764001606"]
["TECHNIK","EDDING 140 S modrá",null,"Permanentní pero s kulatým hrotem 0,3mm / barva modrá","1ks",1.4844999647431258,{"$f":"F2880*(1-Elteq!$F$9)","v":1.4844999647431258},""]
["TECHNIK","EDDING 140 S oranž.",null,"Permanentní pero s kulatým hrotem 0,3mm / barva oranžová","1ks",1.4844999647431258,{"$f":"F2881*(1-Elteq!$F$9)","v":1.4844999647431258},""]
["TECHNIK","EDDING 140 S rudá",null,"Permanentní pero s kulatým hrotem 0,3mm / barva rudá","1ks",1.4844999647431258,{"$f":"F2882*(1-Elteq!$F$9)","v":1.4844999647431258},""]
["TECHNIK","EDDING 140 S žlutá",null,"Permanentní pero s kulatým hrotem 0,3mm / barva žlutá","1ks",1.4844999647431258,{"$f":"F2883*(1-Elteq!$F$9)","v":1.4844999647431258},""]
["TECHNIK","EDDING 141 F černá",null,"Permanentní pero s kulatým hrotem 0,6mm / barva černá","1ks",1.4102749665059695,{"$f":"F2884*(1-Elteq!$F$9)","v":1.4102749665059695},"4004764001330"]
["TECHNIK","EDDING 141 F modrá",null,"Permanentní pero s kulatým hrotem 0,6mm / barva modrá","1ks",1.4102749665059695,{"$f":"F2885*(1-Elteq!$F$9)","v":1.4102749665059695},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"EDDING 141 F oranž",null,"Permanentní pero s kulatým hrotem 0,6mm / barva oranžová","1ks",1.4102749665059695,{"$f":"F2886*(1-Elteq!$F$9)","v":1.4102749665059695},""]
["TECHNIK","EDDING 141 F rudá",null,"Permanentní pero s kulatým hrotem 0,6mm / barva rudá","1ks",1.4102749665059695,{"$f":"F2887*(1-Elteq!$F$9)","v":1.4102749665059695},""]
["TECHNIK","EDDING 141 F zelená",null,"Permanentní pero s kulatým hrotem 0,6mm / barva zelená","1ks",1.4102749665059695,{"$f":"F2888*(1-Elteq!$F$9)","v":1.4102749665059695},""]
["TECHNIK","EDDING 141 F žlutá",null,"Permanentní pero s kulatým hrotem 0,6mm / barva žlutá","1ks",1.4102749665059695,{"$f":"F2889*(1-Elteq!$F$9)","v":1.4102749665059695},""]
["TECHNIK","EDDING 142 M černá",null,"Permanentní pero s kulatým hrotem 1,0mm / barva černá","1ks",1.4102749665059695,{"$f":"F2890*(1-Elteq!$F$9)","v":1.4102749665059695},"4004764000760"]
["TECHNIK","EDDING 142 M fialová",null,"Permanentní pero s kulatým hrotem 1,0mm / barva fialová","1ks",1.4102749665059695,{"$f":"F2891*(1-Elteq!$F$9)","v":1.4102749665059695},""]
["TECHNIK","EDDING 142 M modrá",null,"Permanentní pero s kulatým hrotem 1,0mm / barva modrá","1ks",1.4102749665059695,{"$f":"F2892*(1-Elteq!$F$9)","v":1.4102749665059695},""]
["TECHNIK","EDDING 142 M oranž",null,"Permanentní pero s kulatým hrotem 1,0mm / barva oranžová","1ks",1.4102749665059695,{"$f":"F2893*(1-Elteq!$F$9)","v":1.4102749665059695},""]
["TECHNIK","EDDING 142 M rudá",null,"Permanentní pero s kulatým hrotem 1,0mm / barva rudá","1ks",1.4102749665059695,{"$f":"F2894*(1-Elteq!$F$9)","v":1.4102749665059695},""]
["TECHNIK","EDDING 142 M žlutá",null,"Permanentní pero s kulatým hrotem 1,0mm / barva žlutá","1ks",1.4102749665059695,{"$f":"F2895*(1-Elteq!$F$9)","v":1.4102749665059695},""]
["TECHNIK","EDDING 143 B černá",null,"Permanentní pero se seříznutým hrotem 1,0mm / barva černá","1ks",1.6700624603360166,{"$f":"F2896*(1-Elteq!$F$9)","v":1.6700624603360166},""]
["TECHNIK","EDDING 143 B rudá",null,"Permanentní pero se seříznutým hrotem 1,0mm / barva rudá","1ks",1.6700624603360166,{"$f":"F2897*(1-Elteq!$F$9)","v":1.6700624603360166},""]
["TECHNIK","EDDING 147 S černá",null,"Permanentní pero s kulatým hrotem 0,3mm s integrovanou gumou / barva černá","1ks",1.6700624603360166,{"$f":"F2898*(1-Elteq!$F$9)","v":1.6700624603360166},""]
["TECHNIK","EDDING 147 S modrá",null,"Permanentní pero s kulatým hrotem 0,3mm s integrovanou gumou / barva modrá","1ks",1.6700624603360166,{"$f":"F2899*(1-Elteq!$F$9)","v":1.6700624603360166},""]
["TECHNIK","EDDING 147 S rudá",null,"Permanentní pero s kulatým hrotem 0,3mm s integrovanou gumou / barva rudá","1ks",1.6700624603360166,{"$f":"F2900*(1-Elteq!$F$9)","v":1.6700624603360166},""]
["TECHNIK","EDDING 147 S zelená",null,"Permanentní pero s kulatým hrotem 0,3mm s integrovanou gumou / barva zelená","1ks",1.6700624603360166,{"$f":"F2901*(1-Elteq!$F$9)","v":1.6700624603360166},""]
["TECHNIK","EDDING 149 M černá",null,"Permanentní pero s kulatým hrotem 1,0mm s integrovanou gumou / barva černá","1ks",1.6700624603360166,{"$f":"F2902*(1-Elteq!$F$9)","v":1.6700624603360166},""]
["TECHNIK","EDDING 149 M modrá",null,"Permanentní pero s kulatým hrotem 1,0mm s integrovanou gumou / barva modrá","1ks",1.6700624603360166,{"$f":"F2903*(1-Elteq!$F$9)","v":1.6700624603360166},""]
["TECHNIK","EDDING 149 M rudá",null,"Permanentní pero s kulatým hrotem 1,0mm s integrovanou gumou / barva rudá","1ks",1.6700624603360166,{"$f":"F2904*(1-Elteq!$F$9)","v":1.6700624603360166},""]
["TECHNIK","EDDING 149 M zelená",null,"Permanentní pero s kulatým hrotem 1,0mm s integrovanou gumou / barva zelená","1ks",1.6700624603360166,{"$f":"F2905*(1-Elteq!$F$9)","v":1.6700624603360166},""]
["TECHNIK","EDDING 404 černá",null,"Permanentní pero s kulatým hrotem 0,75mm / barva černá","1ks",2.2267499471146888,{"$f":"F2906*(1-Elteq!$F$9)","v":2.2267499471146888},""]
["TECHNIK","EDDING 750 bílá",null,"Permanentní pero s kulatým hrotem 2-4mm / barva bílá","1ks",4.3050498977550653,{"$f":"F2907*(1-Elteq!$F$9)","v":4.3050498977550653},""]
["TECHNIK","EDDING 750 černá",null,"Permanentní pero s kulatým hrotem 2-4mm / barva černá","1ks",4.3050498977550653,{"$f":"F2908*(1-Elteq!$F$9)","v":4.3050498977550653},""]
["TECHNIK","EDDING 750 fialová",null,"Permanentní pero s kulatým hrotem 2-4mm / barva fialová","1ks",4.3050498977550653,{"$f":"F2909*(1-Elteq!$F$9)","v":4.3050498977550653},""]
["TECHNIK","EDDING 750 modrá",null,"Permanentní pero s kulatým hrotem 2-4mm / barva modrá","1ks",4.3050498977550653,{"$f":"F2910*(1-Elteq!$F$9)","v":4.3050498977550653},""]
["TECHNIK","EDDING 750 rudá",null,"Permanentní pero s kulatým hrotem 2-4mm / barva červená","1ks",4.3050498977550653,{"$f":"F2911*(1-Elteq!$F$9)","v":4.3050498977550653},""]
["TECHNIK","EDDING 750 zelená",null,"Permanentní pero s kulatým hrotem 2-4mm / barva zelená","1ks",4.3050498977550653,{"$f":"F2912*(1-Elteq!$F$9)","v":4.3050498977550653},""]
["TECHNIK","EDDING 750 žlutá",null,"Permanentní pero s kulatým hrotem 2-4mm / barva žlutá","1ks",4.3050498977550653,{"$f":"F2913*(1-Elteq!$F$9)","v":4.3050498977550653},""]
["TECHNIK","EDDING 751 bílá",null,"Permanentní pero s kulatým hrotem 1-2mm / barva bílá (nově EDDING 791 bílá)","1ks",3.7112499118578146,{"$f":"F2914*(1-Elteq!$F$9)","v":3.7112499118578146},""]
["TECHNIK","EDDING 751 černá",null,"Permanentní pero s kulatým hrotem 1-2mm / barva černá (nově EDDING 791 černá)","1ks",3.7112499118578146,{"$f":"F2915*(1-Elteq!$F$9)","v":3.7112499118578146},""]
["TECHNIK","EDDING 780 bílá",null,"Permanentní pero s kulatým hrotem 0,8mm / barva bílá (nově EDDING 792 bílá)","1ks",4.3050498977550653,{"$f":"F2916*(1-Elteq!$F$9)","v":4.3050498977550653},""]
["TECHNIK","EDDING 790 bílá",null,"Permanentní pero s kulatým hrotem 2-4mm / barva bílá (dříve EDDING 750)","1ks",2.8576624321305171,{"$f":"F2917*(1-Elteq!$F$9)","v":2.8576624321305171},"4004764855247"]
["TECHNIK","EDDING 790 černá",null,"Permanentní pero s kulatým hrotem 2-4mm / barva černá (dříve EDDING 750)","1ks",2.8576624321305171,{"$f":"F2918*(1-Elteq!$F$9)","v":2.8576624321305171},""]
["TECHNIK","EDDING 790 modrá",null,"Permanentní pero s kulatým hrotem 2-4mm / barva modrá","1ks",2.8576624321305171,{"$f":"F2919*(1-Elteq!$F$9)","v":2.8576624321305171},""]
["TECHNIK","EDDING 790 rudá",null,"Permanentní pero s kulatým hrotem 2-4mm / barva rudá","1ks",2.8576624321305171,{"$f":"F2920*(1-Elteq!$F$9)","v":2.8576624321305171},""]
["TECHNIK","EDDING 790 stříbrná",null,"Permanentní pero s kulatým hrotem 2-4mm / barva stříbrná","1ks",2.8576624321305171,{"$f":"F2921*(1-Elteq!$F$9)","v":2.8576624321305171},""]
["TECHNIK","EDDING 790 zelená",null,"Permanentní pero s kulatým hrotem 2-4mm / barva zelená","1ks",2.8576624321305171,{"$f":"F2922*(1-Elteq!$F$9)","v":2.8576624321305171},""]
["TECHNIK","EDDING 790 zlatá",null,"Permanentní pero s kulatým hrotem 2-4mm / barva zlatá","1ks",2.8576624321305171,{"$f":"F2923*(1-Elteq!$F$9)","v":2.8576624321305171},""]
["TECHNIK","EDDING 790 žlutá",null,"Permanentní pero s kulatým hrotem 2-4mm / barva žlutá","1ks",2.8576624321305171,{"$f":"F2924*(1-Elteq!$F$9)","v":2.8576624321305171},""]
["TECHNIK","EDDING 791 bílá",null,"Permanentní pero s kulatým hrotem 1-2mm / barva bílá (dříve EDDING 751)","1ks",2.8576624321305171,{"$f":"F2925*(1-Elteq!$F$9)","v":2.8576624321305171},"4004764837816"]
["TECHNIK","EDDING 791 černá",null,"Permanentní pero s kulatým hrotem 1-2mm / barva černá (dříve EDDING 751)","1ks",2.8576624321305171,{"$f":"F2926*(1-Elteq!$F$9)","v":2.8576624321305171},"4004764837618"]
["TECHNIK","EDDING 791 modrá",null,"Permanentní pero s kulatým hrotem 1-2mm / barva modrá","1ks",2.8576624321305171,{"$f":"F2927*(1-Elteq!$F$9)","v":2.8576624321305171},""]
["TECHNIK","EDDING 791 rudá",null,"Permanentní pero s kulatým hrotem 1-2mm / barva rudá","1ks",2.8576624321305171,{"$f":"F2928*(1-Elteq!$F$9)","v":2.8576624321305171},""]
["TECHNIK","EDDING 791 stříbrná",null,"Permanentní pero s kulatým hrotem 1-2mm / barva stříbrná","1ks",2.8576624321305171,{"$f":"F2929*(1-Elteq!$F$9)","v":2.8576624321305171},""]
["TECHNIK","EDDING 791 zelená",null,"Permanentní pero s kulatým hrotem 1-2mm / barva zelená","1ks",2.8576624321305171,{"$f":"F2930*(1-Elteq!$F$9)","v":2.8576624321305171},""]
["TECHNIK","EDDING 791 zlatá",null,"Permanentní pero s kulatým hrotem 1-2mm / barva zlatá","1ks",2.8576624321305171,{"$f":"F2931*(1-Elteq!$F$9)","v":2.8576624321305171},""]
["TECHNIK","EDDING 791 žlutá",null,"Permanentní pero s kulatým hrotem 1-2mm / barva žlutá","1ks",2.8576624321305171,{"$f":"F2932*(1-Elteq!$F$9)","v":2.8576624321305171},""]
["TECHNIK","EDDING 792 bílá",null,"Permanentní pero s kulatým hrotem 0,8mm / barva bílá (dříve EDDING 780 bílá)","1ks",2.8576624321305171,{"$f":"F2933*(1-Elteq!$F$9)","v":2.8576624321305171},"4004764838097"]
["TECHNIK","EDDING 792 černá",null,"Permanentní pero s kulatým hrotem 0,8mm / barva černá (dříve EDDING 780 černá)","1ks",2.8576624321305171,{"$f":"F2934*(1-Elteq!$F$9)","v":2.8576624321305171},"4004764837939"]
["TECHNIK","EDDING 792 modrá",null,"Permanentní pero s kulatým hrotem 0,8mm / barva modrá","1ks",2.8576624321305171,{"$f":"F2935*(1-Elteq!$F$9)","v":2.8576624321305171},"4004764838011"]
["TECHNIK","EDDING 792 rudá",null,"Permanentní pero s kulatým hrotem 0,8mm / barva rudá","1ks",2.8576624321305171,{"$f":"F2936*(1-Elteq!$F$9)","v":2.8576624321305171},"4004764837977"]
["TECHNIK","EDDING 792 stříbrná",null,"Permanentní pero s kulatým hrotem 0,8mm / barva stříbrná","1ks",2.8576624321305171,{"$f":"F2937*(1-Elteq!$F$9)","v":2.8576624321305171},""]
["TECHNIK","EDDING 792 zelená",null,"Permanentní pero s kulatým hrotem 0,8mm / barva zelená","1ks",2.8576624321305171,{"$f":"F2938*(1-Elteq!$F$9)","v":2.8576624321305171},"4004764838059"]
["TECHNIK","EDDING 792 zlatá",null,"Permanentní pero s kulatým hrotem 0,8mm / barva zlatá","1ks",2.8576624321305171,{"$f":"F2939*(1-Elteq!$F$9)","v":2.8576624321305171},""]
["TECHNIK","EDDING 8200 šedá",null,"Permanentní pero s kulatým hrotem 2-4mm na spáry / barva šedá","1ks",4.4534998942293775,{"$f":"F2940*(1-Elteq!$F$9)","v":4.4534998942293775},""]
["TECHNIK","EDDING 8300 černá",null,"Permanentní pero k průmyslovému použití s kulatým hrotem 1,5-3,0mm / barva černá","1ks",2.3009749453518449,{"$f":"F2941*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","EDDING 8400 černá",null,"Permanentní pero na CD, DVD s kulatým hrotem 0,5-1,0mm / barva černá","1ks",2.3009749453518449,{"$f":"F2942*(1-Elteq!$F$9)","v":2.3009749453518449},"4004764782703"]
["TECHNIK","EDDING 8400 modrá",null,"Permanentní pero na CD, DVD s kulatým hrotem 0,5-1,0mm / barva modrá","1ks",2.3009749453518449,{"$f":"F2943*(1-Elteq!$F$9)","v":2.3009749453518449},"4004764827176"]
["TECHNIK","EDDING 8407 mix",null,"Permanentní pero na kabely s kulatým hrotem 0,3mm / barva černá, modrá, červená, zelená","1sada",7.0142623334112697,{"$f":"F2944*(1-Elteq!$F$9)","v":7.0142623334112697},"4004764937400"]
["TECHNIK","EDDING 8500 RW",null,"Nepermanení pero na CD-RW s kulatým hrotem 1,0mm","1ks",2.3009749453518449,{"$f":"F2945*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","EDDING 8750 bílá",null,"Permanentní pero s kulatým hrotem 2-4mm / barva bílá","1ks",4.4534998942293775,{"$f":"F2946*(1-Elteq!$F$9)","v":4.4534998942293775},""]
["TECHNIK","EDDING 8750 černá",null,"Permanentní pero s kulatým hrotem 2-4mm / barva černá","1ks",4.4534998942293775,{"$f":"F2947*(1-Elteq!$F$9)","v":4.4534998942293775},""]
["TECHNIK","EDDING 8750 modrá",null,"Permanentní pero s kulatým hrotem 2-4mm / barva modrá","1ks",4.4534998942293775,{"$f":"F2948*(1-Elteq!$F$9)","v":4.4534998942293775},""]
["TECHNIK","EDDING 8750 rudá",null,"Permanentní pero s kulatým hrotem 2-4mm / barva rudá","1ks",4.4534998942293775,{"$f":"F2949*(1-Elteq!$F$9)","v":4.4534998942293775},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"EDDING 8750 zelená",null,"Permanentní pero s kulatým hrotem 2-4mm / barva zelená","1ks",4.4534998942293775,{"$f":"F2950*(1-Elteq!$F$9)","v":4.4534998942293775},""]
["TECHNIK","EDDING 8750 žlutá",null,"Permanentní pero s kulatým hrotem 2-4mm / barva žlutá","1ks",4.4534998942293775,{"$f":"F2951*(1-Elteq!$F$9)","v":4.4534998942293775},""]
["TECHNIK","EDDING 8850 černá",null,"Permanentní pero s dlouhým hrotem 0,7-1,0mm / barva černá","1ks",3.3401249206720331,{"$f":"F2952*(1-Elteq!$F$9)","v":3.3401249206720331},""]
["TECHNIK","CV-KC 1",null,"Kabelová příchytka černá na hranu plechu 0,7-3,0mm, svazek rovnoběžný s osou plechu","100ks",16.515062107767275,{"$f":"F2953*(1-Elteq!$F$9)","v":16.515062107767275},"8591735034924"]
["TECHNIK","CV-KC 2",null,"Kabelová příchytka černá na hranu plechu 0,7-3,0mm, svazek rovnoběžný mimo osu plechu","100ks",16.700624603360165,{"$f":"F2954*(1-Elteq!$F$9)","v":16.700624603360165},"8591735034948"]
["TECHNIK","CV-KC 3",null,"Kabelová příchytka černá na hranu plechu 0,7-3,0mm, svazek kolmý na podélnou osu plechu","100ks",15.624362128921399,{"$f":"F2955*(1-Elteq!$F$9)","v":15.624362128921399},"8591735034931"]
["TECHNIK","CV-KC 4",null,"Kabelová příchytka černá na hranu plechu 3,0-6,0mm, svazek kolmý na podélnou osu plechu","100ks",29.318874303676736,{"$f":"F2956*(1-Elteq!$F$9)","v":29.318874303676736},"8591735041373"]
["TECHNIK","CV-KC 5",null,"Kabelová příchytka černá na hranu plechu 0,7-3,0mm, svazek kolmý mimo podélnou osu plechu","100ks",15.624362128921399,{"$f":"F2957*(1-Elteq!$F$9)","v":15.624362128921399},"8591735034955"]
["TECHNIK","CV-KC 6",null,"Kabelová příchytka černá na hranu plechu 3,0-6,0mm, svazek rovnoběžný s osou plechu","100ks",28.168386831000813,{"$f":"F2958*(1-Elteq!$F$9)","v":28.168386831000813},"8591735051754"]
["TECHNIK","CV-KC 7",null,"Kabelová příchytka černá na hranu plechu 3,0-6,0mm, svazek rovnoběžný mimo osu plechu","100ks",28.168386831000813,{"$f":"F2959*(1-Elteq!$F$9)","v":28.168386831000813},"8591735051747"]
["TECHNIK","CV-KC 8",null,"Kabelová příchytka černá na hranu plechu 3,0-6,0mm, svazek kolmý mimo podélnou osu plechu","100ks",27.092124356562046,{"$f":"F2960*(1-Elteq!$F$9)","v":27.092124356562046},"8591735051730"]
["TECHNIK","CV-KC11",null,"Kabelová příchytka černá na hranu plechu 0,7-3,0mm, otvor pro uchycení svazku mimo osu plechu","100ks",23.677774437652857,{"$f":"F2961*(1-Elteq!$F$9)","v":23.677774437652857},"8591735051723"]
["TECHNIK","CV-KC13",null,"Kabelová příchytka černá na hranu plechu 0,7-3,0mm, otvor pro uchycení svazku v ose plechu","100ks",23.677774437652857,{"$f":"F2962*(1-Elteq!$F$9)","v":23.677774437652857},"8591735051709"]
["TECHNIK","CV-KC15",null,"Kabelová příchytka černá na hranu plechu 0,7-3,0mm, univerzální všesměrový otvor pro uchycení svazku","100ks",23.677774437652857,{"$f":"F2963*(1-Elteq!$F$9)","v":23.677774437652857},"8591735051686"]
["TECHNIK","CV-KC17",null,"Kabelová příchytka na hranu plechu 0,7-3,0mm s páskou 3,6x160mm, svazek rovnoběžný mimo osu plechu","100ks",23.677774437652857,{"$f":"F2964*(1-Elteq!$F$9)","v":23.677774437652857},"8591735051693"]
["TECHNIK","CV-KC18",null,"Kabelová příchytka na hranu plechu 0,7-3,0mm s páskou 3,6x160mm, svazek rovnoběžný mimo osu plechu","100ks",23.677774437652857,{"$f":"F2965*(1-Elteq!$F$9)","v":23.677774437652857},"8591735051716"]
["TECHNIK","CV-KC19",null,"Kabelová příchytka na hranu plechu 0,7-3,0mm s páskou 3,6x160mm, svazek kolmý na osu plechu","100ks",23.677774437652857,{"$f":"F2966*(1-Elteq!$F$9)","v":23.677774437652857},"8591735036898"]
["TECHNIK","CV-KC20",null,"Kabelová příchytka na hranu plechu 0,7-3,0mm s páskou 3,6x160mm, svazek svislý k ose plechu","100ks",23.677774437652857,{"$f":"F2967*(1-Elteq!$F$9)","v":23.677774437652857},"8591735036904"]
["TECHNIK","FC 0605",null,"Kabelová příchytka samolepicí","100ks",13.991412167703961,{"$f":"F2968*(1-Elteq!$F$9)","v":13.991412167703961},"8591735057022"]
["TECHNIK","KAP 12x12",null,"Kabelová příchytka přírodní 12x12mm samolepicí, pro pásky šíře 3,6mm","100ks",1.8556249559289073,{"$f":"F2969*(1-Elteq!$F$9)","v":1.8556249559289073},"8591735008543"]
["TECHNIK","KAP 19x19",null,"Kabelová příchytka přírodní 19x19mm samolepicí, pro pásky šíře 3,6mm","100ks",5.1586373774823624,{"$f":"F2970*(1-Elteq!$F$9)","v":5.1586373774823624},"8591735008550"]
["TECHNIK","KAP 19x19/2",null,"Kabelová příchytka přírodní 19x19mm samolepicí, pro pásky šíře 3,6mm (balení 50 párů)","100ks",4.7875123862965809,{"$f":"F2971*(1-Elteq!$F$9)","v":4.7875123862965809},"8591735016463"]
["TECHNIK","KAP 20x20",null,"Kabelová příchytka přírodní 20x20mm samolepicí, pro pásky šíře 4,8mm","100ks",6.4946873457511751,{"$f":"F2972*(1-Elteq!$F$9)","v":6.4946873457511751},"8591735026998"]
["TECHNIK","KAP 25x25.",null,"Kabelová příchytka přírodní 25x25mm samolepicí, pro pásky šíře 4,8mm","100ks",6.8658123369369566,{"$f":"F2973*(1-Elteq!$F$9)","v":6.8658123369369566},""]
["TECHNIK","KAP 25x32",null,"Kabelová příchytka přírodní 25x32mm samolepicí, pro pásky šíře 8,0mm  (v páse po 10ks)","100ks",7.236937328122738,{"$f":"F2974*(1-Elteq!$F$9)","v":7.236937328122738},"8591735008116"]
["TECHNIK","KAP 27x27/3M",null,"Kabelová příchytka přírodní 27x27mm samolepicí, pro pásky šíře 4,8mm (MOQ 3000ks)","100ks",19.669624532846417,{"$f":"F2975*(1-Elteq!$F$9)","v":19.669624532846417},""]
["TECHNIK","KAP 28x28",null,"Kabelová příchytka přírodní 28x28mm samolepicí, pro pásky šíře 4,8mm","100ks",6.4946873457511751,{"$f":"F2976*(1-Elteq!$F$9)","v":6.4946873457511751},"8591735008567"]
["TECHNIK","KAP 28x28/2",null,"Kabelová příchytka přírodní 28x28mm samolepicí, pro pásky šíře 4,8mm (balení 50 párů)","100ks",6.1235623545653937,{"$f":"F2977*(1-Elteq!$F$9)","v":6.1235623545653937},"8591735016470"]
["TECHNIK","KAP 30x30",null,"Kabelová příchytka přírodní 29x29mm samolepicí, pro pásky šíře 7,8mm","100ks",8.5358747972729727,{"$f":"F2978*(1-Elteq!$F$9)","v":8.5358747972729727},"8591735027018"]
["TECHNIK","KAP 40x40",null,"Kabelová příchytka přírodní 39x39mm samolepicí, pro pásky šíře 10,5mm","100ks",14.473874656245476,{"$f":"F2979*(1-Elteq!$F$9)","v":14.473874656245476},"8591735023102"]
["TECHNIK","KAPC 12x12",null,"Kabelová příchytka černá 12x12mm samolepicí, pro pásky šíře 3,6mm","100ks",5.0101873810080493,{"$f":"F2980*(1-Elteq!$F$9)","v":5.0101873810080493},"8591735025038"]
["TECHNIK","KAPC 19x19",null,"Kabelová příchytka černá 19x19mm samolepicí, pro pásky šíře 3,6mm","100ks",5.1586373774823624,{"$f":"F2981*(1-Elteq!$F$9)","v":5.1586373774823624},"8591735011581"]
["TECHNIK","KAPC 19x19/2",null,"Kabelová příchytka černá 19x19mm samolepicí, pro pásky šíře 3,6mm (balení 50 párů)","100ks",4.7875123862965809,{"$f":"F2982*(1-Elteq!$F$9)","v":4.7875123862965809},"8591735048457"]
["TECHNIK","KAPC 25x32",null,"Kabelová příchytka černá 25x32mm samolepicí, pro pásky šíře 8,0mm (10 pásků po 10ks)","100ks",7.236937328122738,{"$f":"F2983*(1-Elteq!$F$9)","v":7.236937328122738},"8591735016487"]
["TECHNIK","KAPC 27x27/3M",null,"Kabelová příchytka černá 27x27mm samolepicí, pro pásky šíře 4,8mm (MOQ 1000ks)","100ks",21.154124497589542,{"$f":"F2984*(1-Elteq!$F$9)","v":21.154124497589542},""]
["TECHNIK","KAPC 28x28",null,"Kabelová příchytka černá 28x28mm samolepicí, pro pásky šíře 4,8mm","100ks",6.4946873457511751,{"$f":"F2985*(1-Elteq!$F$9)","v":6.4946873457511751},"8591735011598"]
["TECHNIK","KAPC 28x28/2",null,"Kabelová příchytka černá 28x28mm samolepicí, pro pásky šíře 4,8mm (balení 50 párů)","100ks",6.1235623545653937,{"$f":"F2986*(1-Elteq!$F$9)","v":6.1235623545653937},"8591735048464"]
["TECHNIK","KAPH 5",null,"Kabelová příchytka hmoždinková do otvoru 5mm, pro pásku šíře max. 5,8mm (CH-5)","100ks",5.9379998589725034,{"$f":"F2987*(1-Elteq!$F$9)","v":5.9379998589725034},"8591735053055"]
["TECHNIK","KAPH 6",null,"Kabelová příchytka hmoždinková do otvoru 6mm, pro pásku šíře max. 9,9mm (CH-6)","100ks",6.3091248501582848,{"$f":"F2988*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735046378"]
["TECHNIK","KAPH 8",null,"Kabelová příchytka hmoždinková do otvoru 8mm, pro pásku šíře max. 9,7mm (CH-8)","100ks",3.1545624250791424,{"$f":"F2989*(1-Elteq!$F$9)","v":3.1545624250791424},"8591735009144"]
["TECHNIK","KAPH 9",null,"Kabelová příchytka hmoždinková do otvoru 9mm, pro pásku šíře max. 9,7mm (CH-9)","100ks",3.7112499118578146,{"$f":"F2990*(1-Elteq!$F$9)","v":3.7112499118578146},"8591735013486"]
["TECHNIK","KAPO 4",null,"Kabelová příchytka do otvoru o průměru 4,8mm pro pásky šíře max. 4,0mm","100ks",5.641099866023878,{"$f":"F2991*(1-Elteq!$F$9)","v":5.641099866023878},"8591735009151"]
["TECHNIK","KAPO 8",null,"Kabelová příchytka do otvoru o průměru 6,2mm pro pásky šíře max. 8,1mm","100ks",6.420462347514019,{"$f":"F2992*(1-Elteq!$F$9)","v":6.420462347514019},"8591735009168"]
["TECHNIK","KAPP 15x25",null,"Kabelová příchytka pro ploché kabely, rozměr 15x25mm samolepicí, barva šedá","100ks",8.1276373069686141,{"$f":"F2993*(1-Elteq!$F$9)","v":8.1276373069686141},"8591735027025"]
["TECHNIK","KAPP 20x25",null,"Kabelová příchytka pro ploché kabely, rozměr 20x25mm samolepicí, barva šedá","100ks",8.3874248007986605,{"$f":"F2994*(1-Elteq!$F$9)","v":8.3874248007986605},"8591735026967"]
["TECHNIK","KAPP 25x25",null,"Kabelová příchytka pro ploché kabely, rozměr 25x25mm samolepicí, barva šedá","100ks",9.8348122664232083,{"$f":"F2995*(1-Elteq!$F$9)","v":9.8348122664232083},"8591735027032"]
["TECHNIK","KAPP 30x25",null,"Kabelová příchytka pro ploché kabely, rozměr 30x25mm samolepicí, barva šedá","100ks",11.875999717945007,{"$f":"F2996*(1-Elteq!$F$9)","v":11.875999717945007},"8591735026974"]
["TECHNIK","KAPS 4/4",null,"Kabelové sedlo přírodní pro pásky šíře max. 4,8mm / otvor 4,3mm","1000ks",140.84193415500405,{"$f":"F2997*(1-Elteq!$F$9)","v":140.84193415500405},"8591735050931"]
["TECHNIK","KAPS 4/5",null,"Kabelové sedlo přírodní pro pásky šíře max. 4,8mm / otvor 5,1mm","1000ks",140.84193415500405,{"$f":"F2998*(1-Elteq!$F$9)","v":140.84193415500405},"8591735050924"]
["TECHNIK","KAPS 5",null,"Kabelové sedlo přírodní pro pásky šíře max. 4,8mm / otvor 3,7mm","100ks",3.7483624109763927,{"$f":"F2999*(1-Elteq!$F$9)","v":3.7483624109763927},"8591735009175"]
["TECHNIK","KAPS 5/4,5",null,"Kabelové sedlo přírodní pro pásky šíře max. 4,8mm / otvor 4,5mm","100ks",4.3792748959922214,{"$f":"F3000*(1-Elteq!$F$9)","v":4.3792748959922214},"8591735025007"]
["TECHNIK","KAPS 9",null,"Kabelové sedlo přírodní pro pásky šíře max. 9,0mm / otvor 6,4mm","100ks",4.9730748818894712,{"$f":"F3001*(1-Elteq!$F$9)","v":4.9730748818894712},"8591735009182"]
["TECHNIK","KAPS 9/4,5",null,"Kabelové sedlo přírodní pro pásky šíře max. 9,0mm / otvor 4,5mm","100ks",8.3503123016800824,{"$f":"F3002*(1-Elteq!$F$9)","v":8.3503123016800824},"8591735025014"]
["TECHNIK","KAPS 9/5",null,"Kabelové sedlo přírodní pro pásky šíře max. 9,0mm / otvor 5,0mm","100ks",8.7214372928658648,{"$f":"F3003*(1-Elteq!$F$9)","v":8.7214372928658648},"8591735025021"]
["TECHNIK","KAPSC 5",null,"Kabelové sedlo černé pro pásky šíře max. 4,8mm / otvor 3,7mm","100ks",4.5648373915851117,{"$f":"F3004*(1-Elteq!$F$9)","v":4.5648373915851117},"8591735012618"]
["TECHNIK","KAPSC 5/4,5",null,"Kabelové sedlo černé pro pásky šíře max. 4,8mm / otvor 4,5mm","100ks",7.979187310494301,{"$f":"F3005*(1-Elteq!$F$9)","v":7.979187310494301},"8591735047788"]
["TECHNIK","KAPSC 9",null,"Kabelové sedlo černé pro pásky šíře max. 9,0mm / otvor 6,4mm","100ks",5.8266623616167692,{"$f":"F3006*(1-Elteq!$F$9)","v":5.8266623616167692},"8591735011604"]
["TECHNIK","KAPSC 9/4,5",null,"Kabelové sedlo černé pro pásky šíře max. 9,0mm / otvor 4,5mm","100ks",9.2410122805259576,{"$f":"F3007*(1-Elteq!$F$9)","v":9.2410122805259576},"8591735050870"]
["TECHNIK","LFC2-4,8x200",null,"Kabelová příchytka do otvoru o průměru 5,0mm vč. vázací pásky 4,8x200mm, barva černá","100ks",11.875999717945007,{"$f":"F3008*(1-Elteq!$F$9)","v":11.875999717945007},"8591735046491"]
["TECHNIK","VP CLIP 4,8x150",null,"Kabelová příchytka černá CV-KC3 na hranu plechu o síle 0,7-3mm s vázací páskou 4,8x150mm","500ks",142.32643411974718,{"$f":"F3009*(1-Elteq!$F$9)","v":142.32643411974718},"8591735034405"]
["TECHNIK","SPR  4 PVC",null,"Svazkovací spirála rudá pro průměr svazku 5-20mm, bezhalogenová, použití -15°C až +80°C","50m",27.277686852154936,{"$f":"F3010*(1-Elteq!$F$9)","v":27.277686852154936},"8591735056612"]
["TECHNIK","SPB  4",null,"Svazkovací spirála bílá pro průměr svazku 10-30mm","10m",3.0061124286048297,{"$f":"F3011*(1-Elteq!$F$9)","v":3.0061124286048297},"8591735034894"]
["TECHNIK","SPB  6",null,"Svazkovací spirála bílá pro průměr svazku 12-50mm","10m",3.3772374197906112,{"$f":"F3012*(1-Elteq!$F$9)","v":3.3772374197906112},"8591735034870"]
["TECHNIK","SPB  8",null,"Svazkovací spirála bílá pro průměr svazku 15-60mm","10m",4.2679373986364864,{"$f":"F3013*(1-Elteq!$F$9)","v":4.2679373986364864},"8591735034900"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"SPB 10",null,"Svazkovací spirála bílá pro průměr svazku 20-65mm","10m",5.3070873739566746,{"$f":"F3014*(1-Elteq!$F$9)","v":5.3070873739566746},"8591735034887"]
["TECHNIK","SPB 12",null,"Svazkovací spirála bílá pro průměr svazku 22-70mm","10m",6.383349848395441,{"$f":"F3015*(1-Elteq!$F$9)","v":6.383349848395441},"8591735029111"]
["TECHNIK","SPB 15",null,"Svazkovací spirála bílá pro průměr svazku 25-100mm","10m",8.090524807850036,{"$f":"F3016*(1-Elteq!$F$9)","v":8.090524807850036},"8591735029128"]
["TECHNIK","SPB 20",null,"Svazkovací spirála bílá pro průměr svazku 30-130mm","10m",11.541987225877804,{"$f":"F3017*(1-Elteq!$F$9)","v":11.541987225877804},"8591735034917"]
["TECHNIK","SPC  2",null,"Svazkovací spirála černá pro průměr svazku 3-20mm","10m",1.1133749735573444,{"$f":"F3018*(1-Elteq!$F$9)","v":1.1133749735573444},"8591735008574"]
["TECHNIK","SPC  4",null,"Svazkovací spirála černá pro průměr svazku 5-45mm","10m",1.4844999647431258,{"$f":"F3019*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735008581"]
["TECHNIK","SPC  6",null,"Svazkovací spirála černá pro průměr svazku 7-55mm","10m",2.4123124427075795,{"$f":"F3020*(1-Elteq!$F$9)","v":2.4123124427075795},"8591735008598"]
["TECHNIK","SPC  8",null,"Svazkovací spirála černá pro průměr svazku 8-60mm","10m",2.5978749383004702,{"$f":"F3021*(1-Elteq!$F$9)","v":2.5978749383004702},"8591735008604"]
["TECHNIK","SPC 10",null,"Svazkovací spirála černá pro průměr svazku 10-65mm","10m",3.1545624250791424,{"$f":"F3022*(1-Elteq!$F$9)","v":3.1545624250791424},"8591735008611"]
["TECHNIK","SPC 12",null,"Svazkovací spirála černá pro průměr svazku 12-70mm","10m",4.0823749030435961,{"$f":"F3023*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735008628"]
["TECHNIK","SPC 15",null,"Svazkovací spirála černá pro průměr svazku 16-85mm","10m",6.383349848395441,{"$f":"F3024*(1-Elteq!$F$9)","v":6.383349848395441},"8591735008635"]
["TECHNIK","SPC 20",null,"Svazkovací spirála černá pro průměr svazku 22-130mm","10m",7.7936248149014107,{"$f":"F3025*(1-Elteq!$F$9)","v":7.7936248149014107},"8591735008642"]
["TECHNIK","SPO  2",null,"Svazkovací spirála oranžová pro průměr svazku  1,5-7mm, bezhalogenová, použití -50°C až +85°C","50m",16.21816211481865,{"$f":"F3026*(1-Elteq!$F$9)","v":16.21816211481865},""]
["TECHNIK","SPO  4",null,"Svazkovací spirála oranžová pro průměr svazku   5-20mm, bezhalogenová, použití -50°C až +85°C","25m",14.844999647431258,{"$f":"F3027*(1-Elteq!$F$9)","v":14.844999647431258},""]
["TECHNIK","SPO 10",null,"Svazkovací spirála oranžová pro průměr svazku 10-40mm, bezhalogenová, použití -50°C až +85°C","25m",35.553774155597864,{"$f":"F3028*(1-Elteq!$F$9)","v":35.553774155597864},""]
["TECHNIK","SPP  2",null,"Svazkovací spirála přírodní pro průměr svazku 3-20mm","10m",1.1133749735573444,{"$f":"F3029*(1-Elteq!$F$9)","v":1.1133749735573444},"8591735008659"]
["TECHNIK","SPP  4",null,"Svazkovací spirála přírodní pro průměr svazku 5-45mm","10m",1.4844999647431258,{"$f":"F3030*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735008666"]
["TECHNIK","SPP  6",null,"Svazkovací spirála přírodní pro průměr svazku 7-55mm","10m",2.4123124427075795,{"$f":"F3031*(1-Elteq!$F$9)","v":2.4123124427075795},"8591735008673"]
["TECHNIK","SPP  8",null,"Svazkovací spirála přírodní pro průměr svazku 8-60mm","10m",2.5978749383004702,{"$f":"F3032*(1-Elteq!$F$9)","v":2.5978749383004702},"8591735008680"]
["TECHNIK","SPP 10",null,"Svazkovací spirála přírodní pro průměr svazku 10-65mm","10m",3.1545624250791424,{"$f":"F3033*(1-Elteq!$F$9)","v":3.1545624250791424},"8591735008697"]
["TECHNIK","SPP 12",null,"Svazkovací spirála přírodní pro průměr svazku 12-70mm","10m",4.0823749030435961,{"$f":"F3034*(1-Elteq!$F$9)","v":4.0823749030435961},"8591735008703"]
["TECHNIK","SPP 15",null,"Svazkovací spirála přírodní pro průměr svazku 16-85mm","10m",6.383349848395441,{"$f":"F3035*(1-Elteq!$F$9)","v":6.383349848395441},"8591735008710"]
["TECHNIK","SPP 20",null,"Svazkovací spirála přírodní pro průměr svazku 22-130mm","10m",7.7936248149014107,{"$f":"F3036*(1-Elteq!$F$9)","v":7.7936248149014107},"8591735008727"]
["TECHNIK","W1   8-12",null,"Hadicová spona pozinkovaná, šíře 9mm / rozsah 8-12mm","100ks",8.7585497919844428,{"$f":"F3037*(1-Elteq!$F$9)","v":8.7585497919844428},""]
["TECHNIK","W1  10-16",null,"Hadicová spona pozinkovaná, šíře 9mm / rozsah 10-16mm","100ks",8.9812247866959112,{"$f":"F3038*(1-Elteq!$F$9)","v":8.9812247866959112},"8591735019358"]
["TECHNIK","W1  12-20",null,"Hadicová spona pozinkovaná, šíře 9mm / rozsah 12-20mm","100ks",9.7605872681860522,{"$f":"F3039*(1-Elteq!$F$9)","v":9.7605872681860522},""]
["TECHNIK","W1  16-25",null,"Hadicová spona pozinkovaná, šíře 9mm / rozsah 16-25mm","100ks",10.725512245269083,{"$f":"F3040*(1-Elteq!$F$9)","v":10.725512245269083},""]
["TECHNIK","W1  20-32",null,"Hadicová spona pozinkovaná, šíře 9mm / rozsah 20-32mm","100ks",11.319312231166334,{"$f":"F3041*(1-Elteq!$F$9)","v":11.319312231166334},""]
["TECHNIK","W1  25-40",null,"Hadicová spona pozinkovaná, šíře 9mm / rozsah 25-40mm","100ks",12.098674712656475,{"$f":"F3042*(1-Elteq!$F$9)","v":12.098674712656475},""]
["TECHNIK","W1  32-50",null,"Hadicová spona pozinkovaná, šíře 9mm / rozsah 32-50mm","50ks",6.420462347514019,{"$f":"F3043*(1-Elteq!$F$9)","v":6.420462347514019},""]
["TECHNIK","W1  40-60",null,"Hadicová spona pozinkovaná, šíře 9mm / rozsah 40-60mm","50ks",6.8286998378183785,{"$f":"F3044*(1-Elteq!$F$9)","v":6.8286998378183785},""]
["TECHNIK","W1  50-70",null,"Hadicová spona pozinkovaná, šíře 9mm / rozsah 50-70mm","50ks",7.4224998237156292,{"$f":"F3045*(1-Elteq!$F$9)","v":7.4224998237156292},""]
["TECHNIK","W1  60-80",null,"Hadicová spona pozinkovaná, šíře 9mm / rozsah 60-80mm","50ks",7.7565123157828326,{"$f":"F3046*(1-Elteq!$F$9)","v":7.7565123157828326},""]
["TECHNIK","W2  50-70",null,"Hadicová spona nerezová, šíře 9mm / rozsah 50-70mm","50ks",12.655362199435148,{"$f":"F3047*(1-Elteq!$F$9)","v":12.655362199435148},""]
["TECHNIK","ID 25x15",null,"Identifikační štítek 25x15mm PA","100ks",6.9400373351741136,{"$f":"F3048*(1-Elteq!$F$9)","v":6.9400373351741136},"8591735008499"]
["TECHNIK","ID 40x20",null,"Identifikační štítek 40x20mm PA","100ks",7.3482748254784731,{"$f":"F3049*(1-Elteq!$F$9)","v":7.3482748254784731},"8591735008505"]
["TECHNIK","ID 60x25",null,"Identifikační štítek 60x25mm PA","100ks",8.9812247866959112,{"$f":"F3050*(1-Elteq!$F$9)","v":8.9812247866959112},"8591735008512"]
["TECHNIK","ID 60x50",null,"Identifikační štítek 60x50mm PA","100ks",13.063599689739508,{"$f":"F3051*(1-Elteq!$F$9)","v":13.063599689739508},"8591735008529"]
["TECHNIK","ID 90x20",null,"Identifikační štítek 90x20mm PA","100ks",15.216124638617039,{"$f":"F3052*(1-Elteq!$F$9)","v":15.216124638617039},"8591735008536"]
["TECHNIK","IDM 60x25",null,"Identifikační štítek žlutý 60x25mm PSH    DO VYPRODÁNÍ ZÁSOB","100ks",3.8596999083321273,{"$f":"F3053*(1-Elteq!$F$9)","v":3.8596999083321273},"8591735027834"]
["TECHNIK","IDM120x50",null,"Identifikační štítek žlutý 120x50x3mm s otvory pro uchycení","10ks",6.9771498342926916,{"$f":"F3054*(1-Elteq!$F$9)","v":6.9771498342926916},"8591735056438"]
["TECHNIK","IDST 50x10",null,"Identifikační štítek nerezový z oceli 316, rozměr 47x10,3mm pro nerezovou pásku VPST šíře 4,5mm","50ks",17.9995620725104,{"$f":"F3055*(1-Elteq!$F$9)","v":17.9995620725104},"8591735049645"]
["TECHNIK","IDST 65x10",null,"Identifikační štítek nerezový z oceli 316, rozměr 65x10,3mm pro nerezovou pásku VPST šíře 4,5mm","50ks",20.226312019625091,{"$f":"F3056*(1-Elteq!$F$9)","v":20.226312019625091},"8591735049652"]
["TECHNIK","IDST 90x10",null,"Identifikační štítek nerezový z oceli 316, rozměr 89x9,5mm pro nerezovou pásku šíře 4,5mm","100ks",15.216124638617039,{"$f":"F3057*(1-Elteq!$F$9)","v":15.216124638617039},"8591735016241"]
["TECHNIK","IDST 90x20",null,"Identifikační štítek nerezový z oceli 316, rozměr 89x19mm pro nerezovou pásku šíře 4,5mm","100ks",21.896374479961107,{"$f":"F3058*(1-Elteq!$F$9)","v":21.896374479961107},"8591735016258"]
["TECHNIK","IDST100x10",null,"Identifikační štítek nerezový z oceli 316, rozměr 102x9,5mm pro nerezovou pásku VPST šíře 4,5 - 8mm","100ks",16.329499612174384,{"$f":"F3059*(1-Elteq!$F$9)","v":16.329499612174384},"8591735048471"]
["TECHNIK","IDST130x10",null,"Identifikační štítek nerezový z oceli 316, rozměr 128x10,3mm pro nerezovou pásku VPST šíře 4,5mm","50ks",26.906561860969155,{"$f":"F3060*(1-Elteq!$F$9)","v":26.906561860969155},"8591735049669"]
["TECHNIK","IDST150x10",null,"Identifikační štítek nerezový z oceli 316, rozměr 150x10,3mm pro nerezovou pásku VPST šíře 4,5mm","50ks",28.391061825712281,{"$f":"F3061*(1-Elteq!$F$9)","v":28.391061825712281},"8591735049676"]
["TECHNIK","IDZ 30x 8",null,"Identifikační štítek zavírací rozměr 30x8mm, PE bralen bezhalogenový","100ks",8.1647498060871921,{"$f":"F3062*(1-Elteq!$F$9)","v":8.1647498060871921},"8591735012977"]
["TECHNIK","IDZ 40x15",null,"Identifikační štítek zavírací rozměr 40x16mm, PE bralen bezhalogenový","100ks",9.3523497778816935,{"$f":"F3063*(1-Elteq!$F$9)","v":9.3523497778816935},"8591735013363"]
["TECHNIK","IDZ 50x10",null,"Identifikační štítek zavírací rozměr 50x10mm, PE bralen bezhalogenový","50ks",4.4906123933479556,{"$f":"F3064*(1-Elteq!$F$9)","v":4.4906123933479556},"8591735037000"]
["TECHNIK","IDZ 60x25",null,"Identifikační štítek zavírací rozměr 60x25mm, PE bralen bezhalogenový","50ks",7.1255998307670039,{"$f":"F3065*(1-Elteq!$F$9)","v":7.1255998307670039},"8591735013370"]
["TECHNIK","IDZ KL 50x20",null,"Identifikační klíčenka zavírací 50x20mm s kovovým kroužkem, barva zelená","10ks",1.2989374691502351,{"$f":"F3066*(1-Elteq!$F$9)","v":1.2989374691502351},""]
["TECHNIK","IDZ UNI 50x20",null,"Identifikační štítek zavírací rozměr 50x20mm, PE bralen bezhalogenový","50ks",6.1235623545653937,{"$f":"F3067*(1-Elteq!$F$9)","v":6.1235623545653937},"8591735021689"]
["TECHNIK","GH-29",null,"Kabelová průchodka gumová velikost Pg 29, do plechu max. 3,0mm barva černá","100ks",45.796823912325429,{"$f":"F3068*(1-Elteq!$F$9)","v":45.796823912325429}]
["TECHNIK","PAZ 02KN4",null,"Označovací profil oválný žlutý pro průměr vodiče 1,3-3,0mm, materiál ZEREX bezhalogenový, cívka 200m","200m",576.72823630270443,{"$f":"F3069*(1-Elteq!$F$9)","v":576.72823630270443},""]
["TECHNIK","PAZ 10KN4",null,"Označovací profil oválný žlutý pro průměr vodiče 2,5-5,0mm, materiál ZEREX bezhalogenový, cívka 100m","100m",288.36411815135222,{"$f":"F3070*(1-Elteq!$F$9)","v":288.36411815135222},""]
["TECHNIK","PAZ 20KN4",null,"Označovací profil oválný žlutý pro průměr vodiče 4-10mm, materiál ZEREX bezhalogenový, cívka 50m","50m",287.80743066457353,{"$f":"F3071*(1-Elteq!$F$9)","v":287.80743066457353},""]
["TECHNIK","PFC04221KA4",null,"Karta se štítky 21x4,2mm (balení 25 karet po 21ks)","1sada",30.951824264894174,{"$f":"F3072*(1-Elteq!$F$9)","v":30.951824264894174},""]
["TECHNIK","PFC45080KA9",null,"Karta se štítky 45x80mm barva bílá","1sada",50.213211307436232,{"$f":"F3073*(1-Elteq!$F$9)","v":50.213211307436232},""]
["TECHNIK","PO-04000BN4",null,"Označovací oválný profil na vodiče o průměru 2,2-2,8mm, barva žlutá, cívka 200m","200m",162.7011961358466,{"$f":"F3074*(1-Elteq!$F$9)","v":162.7011961358466},""]
["TECHNIK","PO-04000DN4",null,"Označovací oválný profil na vodiče o průměru 2,2-2,8mm, barva žlutá, cívka 50m","50m",102.87584755669862,{"$f":"F3075*(1-Elteq!$F$9)","v":102.87584755669862},""]
["TECHNIK","PO-04000SN4",null,"Označovací oválný profil na vodiče o průměru 2,2-2,8mm, barva žlutá, návin 4,5m","1ks",12.506912202960836,{"$f":"F3076*(1-Elteq!$F$9)","v":12.506912202960836},""]
["TECHNIK","PO-05000BN4",null,"Označovací oválný profil na vodiče o průměru 2,7-3,5mm, barva žlutá, cívka 200m","200m",207.05063258254748,{"$f":"F3077*(1-Elteq!$F$9)","v":207.05063258254748},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"PO-05000DN4",null,"Označovací oválný profil na vodiče o průměru 2,7-3,5mm, barva žlutá, cívka 40m","40m",92.59568530085248,{"$f":"F3078*(1-Elteq!$F$9)","v":92.59568530085248},""]
["TECHNIK","PO-05000SN4",null,"Označovací oválný profil na vodiče o průměru 2,7-3,5mm, barva žlutá, návin 4,0m","1ks",12.506912202960836,{"$f":"F3079*(1-Elteq!$F$9)","v":12.506912202960836},""]
["TECHNIK","PO-06000BN4",null,"Označovací oválný profil na vodiče o průměru 3,2-4,0mm, barva žlutá, cívka 200m","200m",257.78341887764378,{"$f":"F3080*(1-Elteq!$F$9)","v":257.78341887764378},""]
["TECHNIK","PO-06000BN9",null,"Označovací oválný profil na vodiče o průměru 3,2-4,0mm, barva bílá, cívka 200m","200m",257.78341887764378,{"$f":"F3081*(1-Elteq!$F$9)","v":257.78341887764378},""]
["TECHNIK","PO-06000DN4",null,"Označovací oválný profil na vodiče o průměru 3,2-4,0mm, barva žlutá, cívka 40m","40m",105.8077349870663,{"$f":"F3082*(1-Elteq!$F$9)","v":105.8077349870663},""]
["TECHNIK","PO-06000SN4",null,"Označovací oválný profil na vodiče o průměru 3,2-4,0mm, barva žlutá, návin 3,5m","1ks",12.506912202960836,{"$f":"F3083*(1-Elteq!$F$9)","v":12.506912202960836},""]
["TECHNIK","PO-068TWBN4",null,"Označovací oválný profil na vodiče o průměru 6,8-7,0mm, barva žlutá, cívka 50m","50m",124.36398454635537,{"$f":"F3084*(1-Elteq!$F$9)","v":124.36398454635537},""]
["TECHNIK","PO-06Q10KN4",null,"Označovací děrovaný oválný profil na vodiče o průměru 3,2-4,0mm, barva žlutá, cívka 100m","100m",184.11510812726618,{"$f":"F3085*(1-Elteq!$F$9)","v":184.11510812726618},""]
["TECHNIK","PO-07000DN4",null,"Označovací oválný profil na vodiče o průměru 3,8-4,7mm, barva žlutá, cívka 30m","30m",79.346523115520071,{"$f":"F3086*(1-Elteq!$F$9)","v":79.346523115520071},""]
["TECHNIK","PO-07000SN4",null,"Označovací oválný profil na vodiče o průměru 3,8-4,7mm, barva žlutá, návin 3,5m","1ks",12.506912202960836,{"$f":"F3087*(1-Elteq!$F$9)","v":12.506912202960836},""]
["TECHNIK","PO-08000BN4",null,"Označovací oválný profil na vodiče o průměru 4,6-5,5mm, barva žlutá, cívka 100m","100m",184.89447060875634,{"$f":"F3088*(1-Elteq!$F$9)","v":184.89447060875634},""]
["TECHNIK","POH07060AA0",null,"Nosný pásek pro návlečky 7-8 znaků","100ks",4.2679373986364864,{"$f":"F3089*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","POH12082AA0",null,"Nosný pásek pro návlečky 12-13 znaků","100ks",6.3091248501582848,{"$f":"F3090*(1-Elteq!$F$9)","v":6.3091248501582848},""]
["TECHNIK","POZ02000KN4",null,"Označovací profil oválný žlutý pro průměr vodiče 1,7-2,2mm, materiál ZEREX bezhalogenový, cívka 250m","250m",355.53774155597864,{"$f":"F3091*(1-Elteq!$F$9)","v":355.53774155597864},""]
["TECHNIK","POZ10000SN4",null,"Označovací profil oválný žlutý, materiál ZEREX bezhalogenový, návin 7m","1ks",22.267499471146888,{"$f":"F3092*(1-Elteq!$F$9)","v":22.267499471146888},""]
["TECHNIK","PP+04600SN4",null,"Plastový pásek pro kapsy PM, PTM a pouzdra PT, PTC šíře 4,6mm, návin 17m, barva žlutá","1ks",31.80541174462147,{"$f":"F3093*(1-Elteq!$F$9)","v":31.80541174462147},""]
["TECHNIK","PPA09000SN4",null,"Plastová páska samolepicí šíře 9mm, délka 10m, barva žlutá","1ks",50.287436305673388,{"$f":"F3094*(1-Elteq!$F$9)","v":50.287436305673388},""]
["TECHNIK","COM 2/0",null,"Návlečka bílá pro průměr vodiče 2,0-2,5mm s potiskem \"0\" (30ks na tyčince)","1ks",1.8185124568103292,{"$f":"F3095*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735056148"]
["TECHNIK","COM 2/1",null,"Návlečka bílá pro průměr vodiče 2,0-2,5mm s potiskem \"1\" (30ks na tyčince)","1ks",1.8185124568103292,{"$f":"F3096*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735056155"]
["TECHNIK","COM 2/2",null,"Návlečka bílá pro průměr vodiče 2,0-2,5mm s potiskem \"2\" (30ks na tyčince)","1ks",1.8185124568103292,{"$f":"F3097*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735056162"]
["TECHNIK","COM 2/3",null,"Návlečka bílá pro průměr vodiče 2,0-2,5mm s potiskem \"3\" (30ks na tyčince)","1ks",1.8185124568103292,{"$f":"F3098*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735056179"]
["TECHNIK","COM 2/4",null,"Návlečka bílá pro průměr vodiče 2,0-2,5mm s potiskem \"4\" (30ks na tyčince)","1ks",1.8185124568103292,{"$f":"F3099*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735056186"]
["TECHNIK","COM 2/5",null,"Návlečka bílá pro průměr vodiče 2,0-2,5mm s potiskem \"5\" (30ks na tyčince)","1ks",1.8185124568103292,{"$f":"F3100*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735056193"]
["TECHNIK","COM 2/6",null,"Návlečka bílá pro průměr vodiče 2,0-2,5mm s potiskem \"6\" (30ks na tyčince)","1ks",1.8185124568103292,{"$f":"F3101*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735056209"]
["TECHNIK","COM 2/7",null,"Návlečka bílá pro průměr vodiče 2,0-2,5mm s potiskem \"7\" (30ks na tyčince)","1ks",1.8185124568103292,{"$f":"F3102*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735056216"]
["TECHNIK","COM 2/8",null,"Návlečka bílá pro průměr vodiče 2,0-2,5mm s potiskem \"8\" (30ks na tyčince)","1ks",1.8185124568103292,{"$f":"F3103*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735056223"]
["TECHNIK","COM 2/9",null,"Návlečka bílá pro průměr vodiče 2,0-2,5mm s potiskem \"9\" (30ks na tyčince)","1ks",1.8185124568103292,{"$f":"F3104*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735056230"]
["TECHNIK","COM 2/E",null,"Návlečka bílá pro průměr vodiče 1,9-2,6mm s potiskem \"E\" (10 tyčinek po 30ks)","10ks",18.185124568103291,{"$f":"F3105*(1-Elteq!$F$9)","v":18.185124568103291},"8591735055370"]
["TECHNIK","COM 2/L",null,"Návlečka bílá pro průměr vodiče 1,9-2,6mm s potiskem \"L\" (10 tyčinek po 30ks)","10ks",18.185124568103291,{"$f":"F3106*(1-Elteq!$F$9)","v":18.185124568103291},"8591735055349"]
["TECHNIK","COM 2/N",null,"Návlečka bílá pro průměr vodiče 1,9-2,6mm s potiskem \"N\" (10 tyčinek po 30ks)","10ks",18.185124568103291,{"$f":"F3107*(1-Elteq!$F$9)","v":18.185124568103291},"8591735055356"]
["TECHNIK","COM 2/P",null,"Návlečka bílá pro průměr vodiče 1,9-2,6mm s potiskem \"P\" (10 tyčinek po 30ks)","10ks",18.185124568103291,{"$f":"F3108*(1-Elteq!$F$9)","v":18.185124568103291},"8591735055363"]
["TECHNIK","COM 2/zem",null,"Návlečka bílá pro průměr vodiče 1,9-2,6mm s potiskem \"uzemnění\" (10 tyčinek po 30ks)","10ks",18.185124568103291,{"$f":"F3109*(1-Elteq!$F$9)","v":18.185124568103291},"8591735055387"]
["TECHNIK","COM 3/0",null,"Návlečka bílá pro průměr vodiče 2,7-3,5mm s potiskem \"0\" (30ks na tyčince)","1ks",1.8556249559289073,{"$f":"F3110*(1-Elteq!$F$9)","v":1.8556249559289073},""]
["TECHNIK","COM 3/1",null,"Návlečka bílá pro průměr vodiče 2,7-3,5mm s potiskem \"1\" (30ks na tyčince)","1ks",1.8556249559289073,{"$f":"F3111*(1-Elteq!$F$9)","v":1.8556249559289073},""]
["TECHNIK","COM 3/2",null,"Návlečka bílá pro průměr vodiče 2,7-3,5mm s potiskem \"2\" (30ks na tyčince)","1ks",1.8556249559289073,{"$f":"F3112*(1-Elteq!$F$9)","v":1.8556249559289073},""]
["TECHNIK","COM 3/3",null,"Návlečka bílá pro průměr vodiče 2,7-3,5mm s potiskem \"3\" (30ks na tyčince)","1ks",1.8556249559289073,{"$f":"F3113*(1-Elteq!$F$9)","v":1.8556249559289073},""]
["TECHNIK","COM 3/4",null,"Návlečka bílá pro průměr vodiče 2,7-3,5mm s potiskem \"4\" (30ks na tyčince)","1ks",1.8556249559289073,{"$f":"F3114*(1-Elteq!$F$9)","v":1.8556249559289073},""]
["TECHNIK","COM 3/5",null,"Návlečka bílá pro průměr vodiče 2,7-3,5mm s potiskem \"5\" (30ks na tyčince)","1ks",1.8556249559289073,{"$f":"F3115*(1-Elteq!$F$9)","v":1.8556249559289073},""]
["TECHNIK","COM 3/6",null,"Návlečka bílá pro průměr vodiče 2,7-3,5mm s potiskem \"6\" (30ks na tyčince)","1ks",1.8556249559289073,{"$f":"F3116*(1-Elteq!$F$9)","v":1.8556249559289073},""]
["TECHNIK","COM 3/7",null,"Návlečka bílá pro průměr vodiče 2,7-3,5mm s potiskem \"7\" (30ks na tyčince)","1ks",1.8556249559289073,{"$f":"F3117*(1-Elteq!$F$9)","v":1.8556249559289073},""]
["TECHNIK","COM 3/8",null,"Návlečka bílá pro průměr vodiče 2,7-3,5mm s potiskem \"8\" (30ks na tyčince)","1ks",1.8556249559289073,{"$f":"F3118*(1-Elteq!$F$9)","v":1.8556249559289073},""]
["TECHNIK","COM 3/9",null,"Návlečka bílá pro průměr vodiče 2,7-3,5mm s potiskem \"9\" (30ks na tyčince)","1ks",1.8556249559289073,{"$f":"F3119*(1-Elteq!$F$9)","v":1.8556249559289073},""]
["TECHNIK","COM 3/A",null,"Návlečka bílá pro průměr vodiče 2,7-3,5mm s potiskem \"A\" (30ks na tyčince)","1ks",1.8556249559289073,{"$f":"F3120*(1-Elteq!$F$9)","v":1.8556249559289073},"8591735040208"]
["TECHNIK","COM 3/C",null,"Návlečka bílá pro průměr vodiče 2,7-3,5mm s potiskem \"C\" (30ks na tyčince)","1ks",1.8556249559289073,{"$f":"F3121*(1-Elteq!$F$9)","v":1.8556249559289073},"8591735040215"]
["TECHNIK","COM 3/G",null,"Návlečka bílá pro průměr vodiče 2,7-3,5mm s potiskem \"G\" (30ks na tyčince)","1ks",1.8556249559289073,{"$f":"F3122*(1-Elteq!$F$9)","v":1.8556249559289073},"8591735040222"]
["TECHNIK","COM 3/L",null,"Návlečka bílá pro průměr vodiče 2,7-3,5mm s potiskem \"L\" (30ks na tyčince)","1ks",1.8556249559289073,{"$f":"F3123*(1-Elteq!$F$9)","v":1.8556249559289073},"8591735040239"]
["TECHNIK","COM 3/N",null,"Návlečka bílá pro průměr vodiče 2,7-3,5mm s potiskem \"N\" (30ks na tyčince)","1ks",1.8556249559289073,{"$f":"F3124*(1-Elteq!$F$9)","v":1.8556249559289073},"8591735040246"]
["TECHNIK","COM 3/P",null,"Návlečka bílá pro průměr vodiče 2,7-3,5mm s potiskem \"P\" (30ks na tyčince)","1ks",1.8556249559289073,{"$f":"F3125*(1-Elteq!$F$9)","v":1.8556249559289073},"8591735040253"]
["TECHNIK","COM 3/R",null,"Návlečka bílá pro průměr vodiče 2,7-3,5mm s potiskem \"R\" (30ks na tyčince)","1ks",1.8556249559289073,{"$f":"F3126*(1-Elteq!$F$9)","v":1.8556249559289073},"8591735040260"]
["TECHNIK","COM 3/S",null,"Návlečka bílá pro průměr vodiče 2,7-3,5mm s potiskem \"S\" (30ks na tyčince)","1ks",1.8556249559289073,{"$f":"F3127*(1-Elteq!$F$9)","v":1.8556249559289073},"8591735040277"]
["TECHNIK","COM 3/T",null,"Návlečka bílá pro průměr vodiče 2,7-3,5mm s potiskem \"T\" (30ks na tyčince)","1ks",1.8556249559289073,{"$f":"F3128*(1-Elteq!$F$9)","v":1.8556249559289073},"8591735040284"]
["TECHNIK","COM 4/0",null,"Návlečka bílá pro průměr vodiče 3,0-3,7mm s potiskem \"0\" (30ks na tyčince)","1ks",1.8927374550474854,{"$f":"F3129*(1-Elteq!$F$9)","v":1.8927374550474854},""]
["TECHNIK","COM 4/1",null,"Návlečka bílá pro průměr vodiče 3,0-3,7mm s potiskem \"1\" (30ks na tyčince)","1ks",1.8927374550474854,{"$f":"F3130*(1-Elteq!$F$9)","v":1.8927374550474854},""]
["TECHNIK","COM 4/2",null,"Návlečka bílá pro průměr vodiče 3,0-3,7mm s potiskem \"2\" (30ks na tyčince)","1ks",1.8927374550474854,{"$f":"F3131*(1-Elteq!$F$9)","v":1.8927374550474854},""]
["TECHNIK","COM 4/3",null,"Návlečka bílá pro průměr vodiče 3,0-3,7mm s potiskem \"3\" (30ks na tyčince)","1ks",1.8927374550474854,{"$f":"F3132*(1-Elteq!$F$9)","v":1.8927374550474854},""]
["TECHNIK","COM 4/4",null,"Návlečka bílá pro průměr vodiče 3,0-3,7mm s potiskem \"4\" (30ks na tyčince)","1ks",1.8927374550474854,{"$f":"F3133*(1-Elteq!$F$9)","v":1.8927374550474854},""]
["TECHNIK","COM 4/5",null,"Návlečka bílá pro průměr vodiče 3,0-3,7mm s potiskem \"5\" (30ks na tyčince)","1ks",1.8927374550474854,{"$f":"F3134*(1-Elteq!$F$9)","v":1.8927374550474854},""]
["TECHNIK","COM 4/6",null,"Návlečka bílá pro průměr vodiče 3,0-3,7mm s potiskem \"6\" (30ks na tyčince)","1ks",1.8927374550474854,{"$f":"F3135*(1-Elteq!$F$9)","v":1.8927374550474854},""]
["TECHNIK","COM 4/7",null,"Návlečka bílá pro průměr vodiče 3,0-3,7mm s potiskem \"7\" (30ks na tyčince)","1ks",1.8927374550474854,{"$f":"F3136*(1-Elteq!$F$9)","v":1.8927374550474854},""]
["TECHNIK","COM 4/8",null,"Návlečka bílá pro průměr vodiče 3,0-3,7mm s potiskem \"8\" (30ks na tyčince)","1ks",1.8927374550474854,{"$f":"F3137*(1-Elteq!$F$9)","v":1.8927374550474854},""]
["TECHNIK","COM 4/9",null,"Návlečka bílá pro průměr vodiče 3,0-3,7mm s potiskem \"9\" (30ks na tyčince)","1ks",1.8927374550474854,{"$f":"F3138*(1-Elteq!$F$9)","v":1.8927374550474854},""]
["TECHNIK","COM 5/0",null,"Návlečka bílá pro průměr vodiče 3,6-4,5mm s potiskem \"0\" (30ks na tyčince)","1ks",1.9298499541660636,{"$f":"F3139*(1-Elteq!$F$9)","v":1.9298499541660636},""]
["TECHNIK","COM 5/1",null,"Návlečka bílá pro průměr vodiče 3,6-4,5mm s potiskem \"1\" (30ks na tyčince)","1ks",1.9298499541660636,{"$f":"F3140*(1-Elteq!$F$9)","v":1.9298499541660636},""]
["TECHNIK","COM 5/2",null,"Návlečka bílá pro průměr vodiče 3,6-4,5mm s potiskem \"2\" (30ks na tyčince)","1ks",1.9298499541660636,{"$f":"F3141*(1-Elteq!$F$9)","v":1.9298499541660636},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"COM 5/3",null,"Návlečka bílá pro průměr vodiče 3,6-4,5mm s potiskem \"3\" (30ks na tyčince)","1ks",1.9298499541660636,{"$f":"F3142*(1-Elteq!$F$9)","v":1.9298499541660636},""]
["TECHNIK","COM 5/4",null,"Návlečka bílá pro průměr vodiče 3,6-4,5mm s potiskem \"4\" (30ks na tyčince)","1ks",1.9298499541660636,{"$f":"F3143*(1-Elteq!$F$9)","v":1.9298499541660636},""]
["TECHNIK","COM 5/5",null,"Návlečka bílá pro průměr vodiče 3,6-4,5mm s potiskem \"5\" (30ks na tyčince)","1ks",1.9298499541660636,{"$f":"F3144*(1-Elteq!$F$9)","v":1.9298499541660636},""]
["TECHNIK","COM 5/6",null,"Návlečka bílá pro průměr vodiče 3,6-4,5mm s potiskem \"6\" (30ks na tyčince)","1ks",1.9298499541660636,{"$f":"F3145*(1-Elteq!$F$9)","v":1.9298499541660636},""]
["TECHNIK","COM 5/7",null,"Návlečka bílá pro průměr vodiče 3,6-4,5mm s potiskem \"7\" (30ks na tyčince)","1ks",1.9298499541660636,{"$f":"F3146*(1-Elteq!$F$9)","v":1.9298499541660636},""]
["TECHNIK","COM 5/8",null,"Návlečka bílá pro průměr vodiče 3,6-4,5mm s potiskem \"8\" (30ks na tyčince)","1ks",1.9298499541660636,{"$f":"F3147*(1-Elteq!$F$9)","v":1.9298499541660636},""]
["TECHNIK","COM 5/9",null,"Návlečka bílá pro průměr vodiče 3,6-4,5mm s potiskem \"9\" (30ks na tyčince)","1ks",1.9298499541660636,{"$f":"F3148*(1-Elteq!$F$9)","v":1.9298499541660636},""]
["TECHNIK","COM 6/0",null,"Návlečka bílá pro průměr vodiče 4,5-6,0mm s potiskem \"0\" (30ks na tyčince)","1ks",1.9669624532846417,{"$f":"F3149*(1-Elteq!$F$9)","v":1.9669624532846417},""]
["TECHNIK","COM 6/1",null,"Návlečka bílá pro průměr vodiče 4,5-6,0mm s potiskem \"1\" (30ks na tyčince)","1ks",1.9669624532846417,{"$f":"F3150*(1-Elteq!$F$9)","v":1.9669624532846417},""]
["TECHNIK","COM 6/2",null,"Návlečka bílá pro průměr vodiče 4,5-6,0mm s potiskem \"2\" (30ks na tyčince)","1ks",1.9669624532846417,{"$f":"F3151*(1-Elteq!$F$9)","v":1.9669624532846417},""]
["TECHNIK","COM 6/3",null,"Návlečka bílá pro průměr vodiče 4,5-6,0mm s potiskem \"3\" (30ks na tyčince)","1ks",1.9669624532846417,{"$f":"F3152*(1-Elteq!$F$9)","v":1.9669624532846417},""]
["TECHNIK","COM 6/4",null,"Návlečka bílá pro průměr vodiče 4,5-6,0mm s potiskem \"4\" (30ks na tyčince)","1ks",1.9669624532846417,{"$f":"F3153*(1-Elteq!$F$9)","v":1.9669624532846417},""]
["TECHNIK","COM 6/5",null,"Návlečka bílá pro průměr vodiče 4,5-6,0mm s potiskem \"5\" (30ks na tyčince)","1ks",1.9669624532846417,{"$f":"F3154*(1-Elteq!$F$9)","v":1.9669624532846417},""]
["TECHNIK","COM 6/6",null,"Návlečka bílá pro průměr vodiče 4,5-6,0mm s potiskem \"6\" (30ks na tyčince)","1ks",1.9669624532846417,{"$f":"F3155*(1-Elteq!$F$9)","v":1.9669624532846417},""]
["TECHNIK","COM 6/7",null,"Návlečka bílá pro průměr vodiče 4,5-6,0mm s potiskem \"7\" (30ks na tyčince)","1ks",1.9669624532846417,{"$f":"F3156*(1-Elteq!$F$9)","v":1.9669624532846417},""]
["TECHNIK","COM 6/8",null,"Návlečka bílá pro průměr vodiče 4,5-6,0mm s potiskem \"8\" (30ks na tyčince)","1ks",1.9669624532846417,{"$f":"F3157*(1-Elteq!$F$9)","v":1.9669624532846417},""]
["TECHNIK","COM 6/9",null,"Návlečka bílá pro průměr vodiče 4,5-6,0mm s potiskem \"9\" (30ks na tyčince)","1ks",1.9669624532846417,{"$f":"F3158*(1-Elteq!$F$9)","v":1.9669624532846417},""]
["TECHNIK","COM 6/A",null,"Návlečka bílá pro průměr vodiče 4,5-6,0mm s potiskem \"A\" (30ks na tyčince)","1ks",1.9669624532846417,{"$f":"F3159*(1-Elteq!$F$9)","v":1.9669624532846417},""]
["TECHNIK","COM 6/B",null,"Návlečka bílá pro průměr vodiče 4,5-6,0mm s potiskem \"B\" (30ks na tyčince)","1ks",1.9669624532846417,{"$f":"F3160*(1-Elteq!$F$9)","v":1.9669624532846417},""]
["TECHNIK","COM 6/C",null,"Návlečka bílá pro průměr vodiče 4,5-6,0mm s potiskem \"C\" (30ks na tyčince)","1ks",1.9669624532846417,{"$f":"F3161*(1-Elteq!$F$9)","v":1.9669624532846417},""]
["TECHNIK","COM 6/M",null,"Návlečka bílá pro průměr vodiče 4,5-6,0mm s potiskem \"M\" (30ks na tyčince)","1ks",1.9669624532846417,{"$f":"F3162*(1-Elteq!$F$9)","v":1.9669624532846417},""]
["TECHNIK","COM 6/S",null,"Návlečka bílá pro průměr vodiče 4,5-6,0mm s potiskem \"S\" (30ks na tyčince)","1ks",1.9669624532846417,{"$f":"F3163*(1-Elteq!$F$9)","v":1.9669624532846417},""]
["TECHNIK","COM 6/W",null,"Návlečka bílá pro průměr vodiče 4,5-6,0mm s potiskem \"W\" (30ks na tyčince)","1ks",1.9669624532846417,{"$f":"F3164*(1-Elteq!$F$9)","v":1.9669624532846417},"8591735050689"]
["TECHNIK","COM 6/X",null,"Návlečka bílá pro průměr vodiče 4,5-6,0mm s potiskem \"X\" (30ks na tyčince)","1ks",1.9669624532846417,{"$f":"F3165*(1-Elteq!$F$9)","v":1.9669624532846417},"8591735050696"]
["TECHNIK","COM 9/1",null,"Návlečka bílá pro průměr vodiče 5,8-9,0mm s potiskem \"1\" (50ks v sáčku)","50ks",10.911074740861975,{"$f":"F3166*(1-Elteq!$F$9)","v":10.911074740861975},"8591735051181"]
["TECHNIK","COM 9/2",null,"Návlečka bílá pro průměr vodiče 5,8-9,0mm s potiskem \"2\" (50ks v sáčku)","50ks",10.911074740861975,{"$f":"F3167*(1-Elteq!$F$9)","v":10.911074740861975},"8591735051198"]
["TECHNIK","COM 9/3",null,"Návlečka bílá pro průměr vodiče 5,8-9,0mm s potiskem \"3\" (50ks v sáčku)","50ks",10.911074740861975,{"$f":"F3168*(1-Elteq!$F$9)","v":10.911074740861975},"8591735051204"]
["TECHNIK","COM 9/E",null,"Návlečka bílá pro průměr vodiče 5,8-9,0mm s potiskem \"E\" (50ks v sáčku)","50ks",10.911074740861975,{"$f":"F3169*(1-Elteq!$F$9)","v":10.911074740861975},"8591735051211"]
["TECHNIK","COM 9/P",null,"Návlečka bílá pro průměr vodiče 5,8-9,0mm s potiskem \"P\" (50ks v sáčku)","50ks",10.911074740861975,{"$f":"F3170*(1-Elteq!$F$9)","v":10.911074740861975},"8591735051174"]
["TECHNIK","COM 9/T",null,"Návlečka bílá pro průměr vodiče 5,8-9,0mm s potiskem \"T\" (50ks v sáčku)","50ks",10.911074740861975,{"$f":"F3171*(1-Elteq!$F$9)","v":10.911074740861975},"8591735051228"]
["TECHNIK","MD 02",null,"Kolíčky prázdné pro návlečky PA 02, barva červená","20ks",4.3792748959922214,{"$f":"F3172*(1-Elteq!$F$9)","v":4.3792748959922214},"8591735042189"]
["TECHNIK","MD 02/3 euro 0-9",null,"Kolíčky s návlečkami PA 02 s potiskem \"0\"-\"9\", EURO kódy","10ks",15.958374620988602,{"$f":"F3173*(1-Elteq!$F$9)","v":15.958374620988602},"8591735042202"]
["TECHNIK","MD 02/3 žlutá 0-9",null,"Kolíčky s návlečkami PA 02 s potiskem \"0\"-\"9\", barva žlutá","10ks",15.958374620988602,{"$f":"F3174*(1-Elteq!$F$9)","v":15.958374620988602},"8591735002565"]
["TECHNIK","MD 02/3.4",null,"Kolíčky s návlečkami PA 02 bez potisku, barva žlutá (10x25ks)","10ks",15.958374620988602,{"$f":"F3175*(1-Elteq!$F$9)","v":15.958374620988602},""]
["TECHNIK","MD 02/3.40\"-\"",null,"Kolíček s návlečkami PA 02 s potiskem \"-\", barva žlutá","10ks",15.958374620988602,{"$f":"F3176*(1-Elteq!$F$9)","v":15.958374620988602},"8591735042134"]
["TECHNIK","MD 02/3.40\"+\"",null,"Kolíček s návlečkami PA 02 s potiskem \"+\", barva žlutá","10ks",15.958374620988602,{"$f":"F3177*(1-Elteq!$F$9)","v":15.958374620988602},"8591735042141"]
["TECHNIK","MD 02/3.40\"0\"",null,"Kolíčky s návlečkami PA 02 s potiskem \"0\", barva žlutá (10x25ks)","10ks",15.958374620988602,{"$f":"F3178*(1-Elteq!$F$9)","v":15.958374620988602},"8591735014070"]
["TECHNIK","MD 02/3.40\"1\"",null,"Kolíček s návlečkami PA 02 s potiskem \"1\", barva žlutá","10ks",15.958374620988602,{"$f":"F3179*(1-Elteq!$F$9)","v":15.958374620988602},"8591735014087"]
["TECHNIK","MD 02/3.40\"2\"",null,"Kolíček s návlečkami PA 02 s potiskem \"2\", barva žlutá","10ks",15.958374620988602,{"$f":"F3180*(1-Elteq!$F$9)","v":15.958374620988602},"8591735014094"]
["TECHNIK","MD 02/3.40\"3\"",null,"Kolíček s návlečkami PA 02 s potiskem \"3\", barva žlutá","10ks",15.958374620988602,{"$f":"F3181*(1-Elteq!$F$9)","v":15.958374620988602},"8591735014100"]
["TECHNIK","MD 02/3.40\"4\"",null,"Kolíček s návlečkami PA 02 s potiskem \"4\", barva žlutá","10ks",15.958374620988602,{"$f":"F3182*(1-Elteq!$F$9)","v":15.958374620988602},"8591735014117"]
["TECHNIK","MD 02/3.40\"5\"",null,"Kolíček s návlečkami PA 02 s potiskem \"5\", barva žlutá","10ks",15.958374620988602,{"$f":"F3183*(1-Elteq!$F$9)","v":15.958374620988602},"8591735014124"]
["TECHNIK","MD 02/3.40\"6\"",null,"Kolíček s návlečkami PA 02 s potiskem \"6\", barva žlutá","10ks",15.958374620988602,{"$f":"F3184*(1-Elteq!$F$9)","v":15.958374620988602},"8591735014131"]
["TECHNIK","MD 02/3.40\"7\"",null,"Kolíček s návlečkami PA 02 s potiskem \"7\", barva žlutá","10ks",15.958374620988602,{"$f":"F3185*(1-Elteq!$F$9)","v":15.958374620988602},"8591735014148"]
["TECHNIK","MD 02/3.40\"8\"",null,"Kolíček s návlečkami PA 02 s potiskem \"8\", barva žlutá","10ks",15.958374620988602,{"$f":"F3186*(1-Elteq!$F$9)","v":15.958374620988602},"8591735014155"]
["TECHNIK","MD 02/3.40\"9\"",null,"Kolíček s návlečkami PA 02 s potiskem \"9\", barva žlutá","10ks",15.958374620988602,{"$f":"F3187*(1-Elteq!$F$9)","v":15.958374620988602},"8591735014162"]
["TECHNIK","MD 02/3.40\"A\"",null,"Kolíček s návlečkami PA 02 s potiskem \"A\", barva žlutá","10ks",15.958374620988602,{"$f":"F3188*(1-Elteq!$F$9)","v":15.958374620988602},"8591735042158"]
["TECHNIK","MD 02/3.40\"B\"",null,"Kolíček s návlečkami PA 02 s potiskem \"B\", barva žlutá","10ks",15.958374620988602,{"$f":"F3189*(1-Elteq!$F$9)","v":15.958374620988602},"8591735042165"]
["TECHNIK","MD 02/3.40\"C\"",null,"Kolíček s návlečkami PA 02 s potiskem \"C\", barva žlutá","10ks",15.958374620988602,{"$f":"F3190*(1-Elteq!$F$9)","v":15.958374620988602},"8591735042172"]
["TECHNIK","MD 02/3.40\"E\"",null,"Kolíček s návlečkami PA 02 s potiskem \"E\", barva žlutá","10ks",15.958374620988602,{"$f":"F3191*(1-Elteq!$F$9)","v":15.958374620988602},"8591735045890"]
["TECHNIK","MD 02/3.40\"U\"",null,"Kolíček s návlečkami PA 02 s potiskem \"U\", barva žlutá","10ks",15.958374620988602,{"$f":"F3192*(1-Elteq!$F$9)","v":15.958374620988602},"8591735046880"]
["TECHNIK","MD 02/3.40\"V\"",null,"Kolíček s návlečkami PA 02 s potiskem \"V\", barva žlutá","10ks",15.958374620988602,{"$f":"F3193*(1-Elteq!$F$9)","v":15.958374620988602},"8591735046897"]
["TECHNIK","MD 02/3.40\"W\"",null,"Kolíček s návlečkami PA 02 s potiskem \"W\", barva žlutá","10ks",15.958374620988602,{"$f":"F3194*(1-Elteq!$F$9)","v":15.958374620988602},"8591735046903"]
["TECHNIK","MD 10",null,"Kolíčky prázdné pro návlečky PA 1, barva modrá","20ks",4.3792748959922214,{"$f":"F3195*(1-Elteq!$F$9)","v":4.3792748959922214},"8591735042196"]
["TECHNIK","MD 10/3 žlutá 0-9",null,"Kolíčky s návlečkami PA 1 s potiskem \"0\"-\"9\", barva žlutá","10ks",15.958374620988602,{"$f":"F3196*(1-Elteq!$F$9)","v":15.958374620988602},"8591735015565"]
["TECHNIK","MD 10/3.4",null,"Kolíčky s návlečkami PA 1 bez potisku, barva žlutá (10x25ks)","10ks",15.958374620988602,{"$f":"F3197*(1-Elteq!$F$9)","v":15.958374620988602},""]
["TECHNIK","MD 10/3.40\"-\"",null,"Kolíček s návlečkami PA 1 s potiskem \"-\", barva žlutá","10ks",15.958374620988602,{"$f":"F3198*(1-Elteq!$F$9)","v":15.958374620988602},"8591735042226"]
["TECHNIK","MD 10/3.40\"+\"",null,"Kolíček s návlečkami PA 1 s potiskem \"+\", barva žlutá","10ks",15.958374620988602,{"$f":"F3199*(1-Elteq!$F$9)","v":15.958374620988602},"8591735042233"]
["TECHNIK","MD 10/3.40\"0\"",null,"Kolíček s návlečkami PA 1 s potiskem \"0\", barva žlutá","10ks",15.958374620988602,{"$f":"F3200*(1-Elteq!$F$9)","v":15.958374620988602},""]
["TECHNIK","MD 10/3.40\"1\"",null,"Kolíček s návlečkami PA 1 s potiskem \"1\", barva žlutá","10ks",15.958374620988602,{"$f":"F3201*(1-Elteq!$F$9)","v":15.958374620988602},""]
["TECHNIK","MD 10/3.40\"2\"",null,"Kolíček s návlečkami PA 1 s potiskem \"2\", barva žlutá","10ks",15.958374620988602,{"$f":"F3202*(1-Elteq!$F$9)","v":15.958374620988602},""]
["TECHNIK","MD 10/3.40\"3\"",null,"Kolíček s návlečkami PA 1 s potiskem \"3\", barva žlutá","10ks",15.958374620988602,{"$f":"F3203*(1-Elteq!$F$9)","v":15.958374620988602},""]
["TECHNIK","MD 10/3.40\"4\"",null,"Kolíček s návlečkami PA 1 s potiskem \"4\", barva žlutá","10ks",15.958374620988602,{"$f":"F3204*(1-Elteq!$F$9)","v":15.958374620988602},""]
["TECHNIK","MD 10/3.40\"5\"",null,"Kolíček s návlečkami PA 1 s potiskem \"5\", barva žlutá","10ks",15.958374620988602,{"$f":"F3205*(1-Elteq!$F$9)","v":15.958374620988602},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"MD 10/3.40\"6\"",null,"Kolíček s návlečkami PA 1 s potiskem \"6\", barva žlutá","10ks",15.958374620988602,{"$f":"F3206*(1-Elteq!$F$9)","v":15.958374620988602},""]
["TECHNIK","MD 10/3.40\"7\"",null,"Kolíček s návlečkami PA 1 s potiskem \"7\", barva žlutá","10ks",15.958374620988602,{"$f":"F3207*(1-Elteq!$F$9)","v":15.958374620988602},""]
["TECHNIK","MD 10/3.40\"8\"",null,"Kolíček s návlečkami PA 1 s potiskem \"8\", barva žlutá","10ks",15.958374620988602,{"$f":"F3208*(1-Elteq!$F$9)","v":15.958374620988602},""]
["TECHNIK","MD 10/3.40\"9\"",null,"Kolíček s návlečkami PA 1 s potiskem \"9\", barva žlutá","10ks",15.958374620988602,{"$f":"F3209*(1-Elteq!$F$9)","v":15.958374620988602},""]
["TECHNIK","MD 10/3.40\"A\"",null,"Kolíček s návlečkami PA 1 s potiskem \"A\", barva žlutá","10ks",15.958374620988602,{"$f":"F3210*(1-Elteq!$F$9)","v":15.958374620988602},"8591735040437"]
["TECHNIK","MD 10/3.40\"C\"",null,"Kolíček s návlečkami PA 1 s potiskem \"C\", barva žlutá","10ks",15.958374620988602,{"$f":"F3211*(1-Elteq!$F$9)","v":15.958374620988602},"8591735040390"]
["TECHNIK","MD 10/3.40\"G\"",null,"Kolíček s návlečkami PA 1 s potiskem \"G\", barva žlutá","10ks",15.958374620988602,{"$f":"F3212*(1-Elteq!$F$9)","v":15.958374620988602},"8591735040413"]
["TECHNIK","MD 10/3.40\"H\"",null,"Kolíček s návlečkami PA 1 s potiskem \"H\", barva žlutá","10ks",15.958374620988602,{"$f":"F3213*(1-Elteq!$F$9)","v":15.958374620988602},"8591735042219"]
["TECHNIK","MD 10/3.40\"L\"",null,"Kolíček s návlečkami PA 1 s potiskem \"L\", barva žlutá","10ks",15.958374620988602,{"$f":"F3214*(1-Elteq!$F$9)","v":15.958374620988602},"8591735040420"]
["TECHNIK","MD 10/3.40\"N\"",null,"Kolíček s návlečkami PA 1 s potiskem \"N\", barva žlutá","10ks",15.958374620988602,{"$f":"F3215*(1-Elteq!$F$9)","v":15.958374620988602},"8591735040444"]
["TECHNIK","MD 10/3.40\"R\"",null,"Kolíček s návlečkami PA 1 s potiskem \"R\", barva žlutá","10ks",15.958374620988602,{"$f":"F3216*(1-Elteq!$F$9)","v":15.958374620988602},"8591735040406"]
["TECHNIK","MD 10/3.40\"S\"",null,"Kolíček s návlečkami PA 1 s potiskem \"S\", barva žlutá","10ks",15.958374620988602,{"$f":"F3217*(1-Elteq!$F$9)","v":15.958374620988602},"8591735040383"]
["TECHNIK","MD 10/3.40\"U\"",null,"Kolíček s návlečkami PA 1 s potiskem \"U\", barva žlutá","10ks",15.958374620988602,{"$f":"F3218*(1-Elteq!$F$9)","v":15.958374620988602},"8591735042240"]
["TECHNIK","MD 10/3.40\"V\"",null,"Kolíček s návlečkami PA 1 s potiskem \"V\", barva žlutá","10ks",15.958374620988602,{"$f":"F3219*(1-Elteq!$F$9)","v":15.958374620988602},"8591735042257"]
["TECHNIK","MD 10/3.40\"W\"",null,"Kolíček s návlečkami PA 1 s potiskem \"W\", barva žlutá","10ks",15.958374620988602,{"$f":"F3220*(1-Elteq!$F$9)","v":15.958374620988602},"8591735042264"]
["TECHNIK","MD 10/6.40\"PE\"",null,"Kolíček s návlečkami PA 1 s potiskem \"PE\", barva žlutá","10ks",15.958374620988602,{"$f":"F3221*(1-Elteq!$F$9)","v":15.958374620988602},"8591735040451"]
["TECHNIK","MDH 2002",null,"Otočný aplikátor pro kolíčky s návlečkami PA 02 červený (prázdný)","1ks",12.61824970031657,{"$f":"F3222*(1-Elteq!$F$9)","v":12.61824970031657},""]
["TECHNIK","MDH 2002 K",null,"Otočný aplikátor s kolíčky a návlečkami PA 02 červený","1sada",44.163873951107995,{"$f":"F3223*(1-Elteq!$F$9)","v":44.163873951107995},""]
["TECHNIK","MDH 2010",null,"Otočný aplikátor pro kolíčky s návlečkami PA 1 modrý (prázdný)","1ks",12.61824970031657,{"$f":"F3224*(1-Elteq!$F$9)","v":12.61824970031657},""]
["TECHNIK","MDH 2010 K",null,"Otočný aplikátor s kolíčky a návlečkami PA 1 modrý","1sada",44.163873951107995,{"$f":"F3225*(1-Elteq!$F$9)","v":44.163873951107995},""]
["TECHNIK","PAD-3M",null,"Jehla - montážní nerezová pomůska pro navlékání návleček PA 02","1ks",9.9832622628975205,{"$f":"F3226*(1-Elteq!$F$9)","v":9.9832622628975205},""]
["TECHNIK","PAD-4M",null,"Jehla - montážní nerezová pomůska pro navlékání návleček PA 1","1ks",9.9832622628975205,{"$f":"F3227*(1-Elteq!$F$9)","v":9.9832622628975205},""]
["TECHNIK","P A  1,0 P",null,"Navlékací profil na vodič o průměru 1,0-2,0mm (průřez 0,2-1,5mm2) Profi (cena za 200m)","200m",429.02048981076337,{"$f":"F3228*(1-Elteq!$F$9)","v":429.02048981076337},"8591735041601"]
["TECHNIK","P A  1,5",null,"Navlékací profil 4x4mm na vodič o průměru 2,0-3,5mm (průřez 0,5-1,5mm2) Kapro (POB)","100m",16.143937116581494,{"$f":"F3229*(1-Elteq!$F$9)","v":16.143937116581494},"8591735009366"]
["TECHNIK","P A  1,5 P",null,"Navlékací profil 5x5mm na vodič o průměru 2,0-4,0mm (průřez 0,35-1,5mm2) balení 2kg=111,2m","110m",23.269536947348499,{"$f":"F3230*(1-Elteq!$F$9)","v":23.269536947348499},"8591735054205"]
["TECHNIK","P A  1,5 SET",null,"Sada 200ks návleček délky 35mm pro průřez 0,5-1,5mm2 + permanentní pero s hrotem 0,6mm","1sada",4.824624885415159,{"$f":"F3231*(1-Elteq!$F$9)","v":4.824624885415159},"8591735021115"]
["TECHNIK","P A  2,5",null,"Navlékací profil 5x5mm na vodič o průměru 2,5-4,0mm (průřez 1,5-2,5mm2) Kapro (POB)","100m",23.195311949111343,{"$f":"F3232*(1-Elteq!$F$9)","v":23.195311949111343},"8591735009373"]
["TECHNIK","P A  2,5 P",null,"Navlékací profil 5x5mm na vodič o průměru 2,5-4,5mm (průřez 0,75-2,5mm2) balení 2kg=118,7m","110m",25.310724398870295,{"$f":"F3233*(1-Elteq!$F$9)","v":25.310724398870295},"8591735054229"]
["TECHNIK","P A  2,5 SET",null,"Sada 200ks návleček délky 35mm pro průřez 1,5-2,5mm2 + permanentní pero s hrotem 0,6mm","1sada",5.1957498766009405,{"$f":"F3234*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735021108"]
["TECHNIK","P A  4",null,"Navlékací profil 6x6mm na vodič o průměru 3,5-5,0mm (průřez 2,5-4,0mm2) Kapro (POB)","100m",32.844561719941659,{"$f":"F3235*(1-Elteq!$F$9)","v":32.844561719941659},"8591735009380"]
["TECHNIK","P A  4 P",null,"Navlékací profil 6x6mm na vodič o průměru 3,0-5,0mm (průřez 1,5-4,0mm2) balení 3kg=125,1m","125m",40.823749030435962,{"$f":"F3236*(1-Elteq!$F$9)","v":40.823749030435962},"8591735041595"]
["TECHNIK","P A  4 SET",null,"Sada 100ks návleček délky 35mm pro průřez 2,5-4,0mm2 + permanentní pero s hrotem 0,6mm","1sada",4.824624885415159,{"$f":"F3237*(1-Elteq!$F$9)","v":4.824624885415159},"8591735021122"]
["TECHNIK","P A  6",null,"Navlékací profil na vodič o průměru 5,0-6,0mm (průřez 6,0mm2) Kapro","100m",37.112499118578143,{"$f":"F3238*(1-Elteq!$F$9)","v":37.112499118578143},"8591735052836"]
["TECHNIK","P A  6 P",null,"Navlékací profil 8x7mm na vodič o průměru 3,5-6,0mm (průřez 4-6mm2) balení 3kg=85,8m","85m",34.700186675870569,{"$f":"F3239*(1-Elteq!$F$9)","v":34.700186675870569},"8591735049256"]
["TECHNIK","P A  6 SET",null,"Sada 50ks návleček délky 35mm pro průřez 4-6mm2 + permanentní pero s hrotem 0,6mm","1sada",5.1957498766009405,{"$f":"F3240*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735029630"]
["TECHNIK","P A 10",null,"Navlékací profil na vodič o průměru 7,0-8,0mm (průřez 10mm2) Kapro","50m",23.380874444704233,{"$f":"F3241*(1-Elteq!$F$9)","v":23.380874444704233},"8591735052843"]
["TECHNIK","P A 10 P",null,"Navlékací profil 9x8mm na vodič o průměru 4,5-8,0mm (průřez 6-10mm2) balení 5kg=131,5m","130m",60.790273556231,{"$f":"F3242*(1-Elteq!$F$9)","v":60.790273556231},"8591735049263"]
["TECHNIK","P A 10 SET",null,"Sada 50ks návleček délky 35mm pro průřez 6-10mm2 + permanentní pero s hrotem 0,6mm","1sada",5.5668748677867219,{"$f":"F3243*(1-Elteq!$F$9)","v":5.5668748677867219},"8591735029647"]
["TECHNIK","P A 16",null,"Navlékací profil na vodič o průměru 8,5-9,5mm (průřez 16mm2) Kapro","50m",29.318874303676736,{"$f":"F3244*(1-Elteq!$F$9)","v":29.318874303676736},"8591735052850"]
["TECHNIK","P A 16 P",null,"Navlékací profil 9x7mm na vodič o průměru 4,0-10mm (průřez 6-16mm2) Profi","50m",178.88224575154666,{"$f":"F3245*(1-Elteq!$F$9)","v":178.88224575154666},"8591735041588"]
["TECHNIK","P A 25 P",null,"Navlékací profil 11x11mm na vodič o průměru 6,0-12mm (průřez 10-25mm2) balení 5kg=77m","75m",61.235623545653944,{"$f":"F3246*(1-Elteq!$F$9)","v":61.235623545653944},"8591735054243"]
["TECHNIK","P A 25 SET",null,"Sada 50ks návleček délky 35mm pro průřez 10-25mm2 + permanentní pero s hrotem 0,6mm","1sada",5.5668748677867219,{"$f":"F3247*(1-Elteq!$F$9)","v":5.5668748677867219},"8591735054250"]
["TECHNIK","P A 70 P",null,"Navlékací profil 16x11mm na vodič o průměru 8,0-16mm (průřez 16-70mm2) Profi","25m",202.63424518743668,{"$f":"F3248*(1-Elteq!$F$9)","v":202.63424518743668},"8591735041618"]
["TECHNIK","PA 02/12",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 12mm, bez potisku, žlutá","100ks",5.0844123792452063,{"$f":"F3249*(1-Elteq!$F$9)","v":5.0844123792452063},""]
["TECHNIK","PA 02/15",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 15mm, bez potisku, žlutá","100ks",7.6080623193085195,{"$f":"F3250*(1-Elteq!$F$9)","v":7.6080623193085195},""]
["TECHNIK","PA 02/21",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 21mm, bez potisku, žlutá","100ks",7.5709498201899414,{"$f":"F3251*(1-Elteq!$F$9)","v":7.5709498201899414},""]
["TECHNIK","PA 02/3",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, bez potisku, žlutá","200ks",3.265899922434877,{"$f":"F3252*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3 euro 0-9",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"0-9\", EURO kódy","200ks",6.1977873528025507,{"$f":"F3253*(1-Elteq!$F$9)","v":6.1977873528025507},"8591735040345"]
["TECHNIK","PA 02/3 žlutá 0-9",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"0-9\", žlutá","200ks",6.1977873528025507,{"$f":"F3254*(1-Elteq!$F$9)","v":6.1977873528025507},"8591735040352"]
["TECHNIK","PA 02/3.09 \"+\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"+\", černá","200ks",3.265899922434877,{"$f":"F3255*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.09 \"0\"euro",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"0\", černá","200ks",3.265899922434877,{"$f":"F3256*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.09 \"1\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"1\", černá","200ks",3.265899922434877,{"$f":"F3257*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.09 \"2\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"2\", černá","200ks",3.265899922434877,{"$f":"F3258*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.09 \"3\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"3\", černá","200ks",3.265899922434877,{"$f":"F3259*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.09 \"4\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"4\", černá","200ks",3.265899922434877,{"$f":"F3260*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.09 \"5\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"5\", černá","200ks",3.265899922434877,{"$f":"F3261*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.09 \"G\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"G\", černá","200ks",3.265899922434877,{"$f":"F3262*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.09 \"L\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"L\", černá","200ks",3.265899922434877,{"$f":"F3263*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.19 \"1\"euro",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"1\", hnědá","200ks",3.265899922434877,{"$f":"F3264*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.29 \"+\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"+\", červená","200ks",3.265899922434877,{"$f":"F3265*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.29 \"2\"euro",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"2\", červená","200ks",3.265899922434877,{"$f":"F3266*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.30 \"3\"euro",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"3\", oranžová","200ks",3.265899922434877,{"$f":"F3267*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.4. 500",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, bez potisku, žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3268*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 02/3.40 \"-\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"-\", žlutá","200ks",3.265899922434877,{"$f":"F3269*(1-Elteq!$F$9)","v":3.265899922434877},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"PA 02/3.40 \"-\" 1000",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"-\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3270*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 02/3.40 \"-\" 500",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"-\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3271*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 02/3.40 \".\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \".\", žlutá","200ks",3.265899922434877,{"$f":"F3272*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.40 \"/\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"/\", žlutá","200ks",3.265899922434877,{"$f":"F3273*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.40 \":\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \":\", žlutá","200ks",3.265899922434877,{"$f":"F3274*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.40 \"+\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"+\", žlutá","200ks",3.265899922434877,{"$f":"F3275*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.40 \"+\" 1000",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"+\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3276*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 02/3.40 \"+\" 500",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"+\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3277*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 02/3.40 \"0\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"0\", žlutá","200ks",3.265899922434877,{"$f":"F3278*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000120"]
["TECHNIK","PA 02/3.40 \"0\" 1000",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"0\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3279*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 02/3.40 \"0\" 500",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"0\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3280*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 02/3.40 \"1\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"1\", žlutá","200ks",3.265899922434877,{"$f":"F3281*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000137"]
["TECHNIK","PA 02/3.40 \"1\" 1000",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"1\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3282*(1-Elteq!$F$9)","v":16.626399605123009},"7330417008560"]
["TECHNIK","PA 02/3.40 \"1\" 500",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"1\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3283*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 02/3.40 \"2\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"2\", žlutá","200ks",3.265899922434877,{"$f":"F3284*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000144"]
["TECHNIK","PA 02/3.40 \"2\" 1000",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"2\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3285*(1-Elteq!$F$9)","v":16.626399605123009},"7330417008577"]
["TECHNIK","PA 02/3.40 \"2\" 500",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"2\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3286*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 02/3.40 \"3\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"3\", žlutá","200ks",3.265899922434877,{"$f":"F3287*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000151"]
["TECHNIK","PA 02/3.40 \"3\" 1000",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"3\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3288*(1-Elteq!$F$9)","v":16.626399605123009},"7330417008584"]
["TECHNIK","PA 02/3.40 \"3\" 500",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"3\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3289*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 02/3.40 \"4\" 1000",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"4\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3290*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 02/3.40 \"4\" 500",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"4\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3291*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 02/3.40 \"4\"euro",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"4\", žlutá","200ks",3.265899922434877,{"$f":"F3292*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000168"]
["TECHNIK","PA 02/3.40 \"5\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"5\", žlutá","200ks",3.265899922434877,{"$f":"F3293*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000175"]
["TECHNIK","PA 02/3.40 \"5\" 1000",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"5\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3294*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 02/3.40 \"5\" 500",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"5\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3295*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 02/3.40 \"6\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"6\", žlutá","200ks",3.265899922434877,{"$f":"F3296*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000182"]
["TECHNIK","PA 02/3.40 \"6\" 1000",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"6\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3297*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 02/3.40 \"6\" 500",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"6\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3298*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 02/3.40 \"7\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"7\", žlutá","200ks",3.265899922434877,{"$f":"F3299*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000199"]
["TECHNIK","PA 02/3.40 \"7\" 1000",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"7\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3300*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 02/3.40 \"7\" 500",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"7\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3301*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 02/3.40 \"8\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"8\", žlutá","200ks",3.265899922434877,{"$f":"F3302*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000205"]
["TECHNIK","PA 02/3.40 \"8\" 1000",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"8\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3303*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 02/3.40 \"8\" 250",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"8\", žlutá (250ks)","250ks",4.2679373986364864,{"$f":"F3304*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PA 02/3.40 \"8\" 500",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"8\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3305*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 02/3.40 \"9\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"9\", žlutá","200ks",3.265899922434877,{"$f":"F3306*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000212"]
["TECHNIK","PA 02/3.40 \"9\" 1000",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"9\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3307*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 02/3.40 \"9\" 250",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"9\", žlutá (250ks)","250ks",4.2679373986364864,{"$f":"F3308*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PA 02/3.40 \"9\" 500",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"9\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3309*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 02/3.40 \"A\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"A\", žlutá","200ks",3.265899922434877,{"$f":"F3310*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000229"]
["TECHNIK","PA 02/3.40 \"A\" 1000",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"A\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3311*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 02/3.40 \"B\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"B\", žlutá","200ks",3.265899922434877,{"$f":"F3312*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.40 \"C\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"C\", žlutá","200ks",3.265899922434877,{"$f":"F3313*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000243"]
["TECHNIK","PA 02/3.40 \"D\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"D\", žlutá","200ks",3.265899922434877,{"$f":"F3314*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.40 \"E\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"E\", žlutá","200ks",3.265899922434877,{"$f":"F3315*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000267"]
["TECHNIK","PA 02/3.40 \"F\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"F\", žlutá","200ks",3.265899922434877,{"$f":"F3316*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.40 \"G\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"G\", žlutá","200ks",3.265899922434877,{"$f":"F3317*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.40 \"H\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"H\", žlutá","200ks",3.265899922434877,{"$f":"F3318*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.40 \"I\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"I\", žlutá","200ks",3.265899922434877,{"$f":"F3319*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.40 \"J\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"J\", žlutá","200ks",3.265899922434877,{"$f":"F3320*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.40 \"K\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"K\", žlutá","200ks",3.265899922434877,{"$f":"F3321*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.40 \"L\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"L\", žlutá","200ks",3.265899922434877,{"$f":"F3322*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000342"]
["TECHNIK","PA 02/3.40 \"M\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"M\", žlutá","200ks",3.265899922434877,{"$f":"F3323*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000359"]
["TECHNIK","PA 02/3.40 \"N\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"N\", žlutá","200ks",3.265899922434877,{"$f":"F3324*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000366"]
["TECHNIK","PA 02/3.40 \"O\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"O\", žlutá","200ks",3.265899922434877,{"$f":"F3325*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.40 \"P\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"P\", žlutá","200ks",3.265899922434877,{"$f":"F3326*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.40 \"Q\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"Q\", žlutá","200ks",3.265899922434877,{"$f":"F3327*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000397"]
["TECHNIK","PA 02/3.40 \"R\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"R\", žlutá","200ks",3.265899922434877,{"$f":"F3328*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000403"]
["TECHNIK","PA 02/3.40 \"S\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"S\", žlutá","200ks",3.265899922434877,{"$f":"F3329*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000410"]
["TECHNIK","PA 02/3.40 \"T\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"T\", žlutá","200ks",3.265899922434877,{"$f":"F3330*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000427"]
["TECHNIK","PA 02/3.40 \"T\" 1000",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"T\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3331*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 02/3.40 \"U\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"U\", žlutá","200ks",3.265899922434877,{"$f":"F3332*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.40 \"U\" 1000",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"U\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3333*(1-Elteq!$F$9)","v":16.626399605123009},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"PA 02/3.40 \"V\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"V\", žlutá","200ks",3.265899922434877,{"$f":"F3334*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000441"]
["TECHNIK","PA 02/3.40 \"V\" 1000",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"V\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3335*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 02/3.40 \"W\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"W\", žlutá","200ks",3.265899922434877,{"$f":"F3336*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.40 \"W\" 1000",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"W\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3337*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 02/3.40 \"X\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"X\", žlutá","200ks",3.265899922434877,{"$f":"F3338*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000465"]
["TECHNIK","PA 02/3.40 \"Y\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"Y\", žlutá","200ks",3.265899922434877,{"$f":"F3339*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000472"]
["TECHNIK","PA 02/3.40 \"Z\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"Z\", žlutá","200ks",3.265899922434877,{"$f":"F3340*(1-Elteq!$F$9)","v":3.265899922434877},"7330417000489"]
["TECHNIK","PA 02/3.40 \"zem\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"zem\", žlutá","200ks",3.265899922434877,{"$f":"F3341*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.59 \"5\"euro",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"5\", zelená","200ks",3.265899922434877,{"$f":"F3342*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.69 \"-\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"-\", modrá","200ks",3.265899922434877,{"$f":"F3343*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.69 \"6\"euro",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"6\", modrá","200ks",3.265899922434877,{"$f":"F3344*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.69 \"N\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"N\", modrá","200ks",3.265899922434877,{"$f":"F3345*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.79 \"7\"euro",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"7\", fialová","200ks",3.265899922434877,{"$f":"F3346*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.8",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, bez potisku, šedá","200ks",3.265899922434877,{"$f":"F3347*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.80 \"8\"euro",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"8\", šedá","200ks",3.265899922434877,{"$f":"F3348*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.90 \"1\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"1\", bílá","200ks",3.265899922434877,{"$f":"F3349*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.90 \"2\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"2\", bílá","200ks",3.265899922434877,{"$f":"F3350*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.90 \"3\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"3\", bílá","200ks",3.265899922434877,{"$f":"F3351*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.90 \"4\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"4\", bílá","200ks",3.265899922434877,{"$f":"F3352*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.90 \"5\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"5\", bílá","200ks",3.265899922434877,{"$f":"F3353*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.90 \"6\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"6\", bílá","200ks",3.265899922434877,{"$f":"F3354*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.90 \"7\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"7\", bílá","200ks",3.265899922434877,{"$f":"F3355*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.90 \"8\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"8\", bílá","200ks",3.265899922434877,{"$f":"F3356*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/3.90 \"9\"euro",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 3mm, s potiskem \"9\", bílá","200ks",3.265899922434877,{"$f":"F3357*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 02/6",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 6mm, bez potisku, žlutá","100ks",4.6390623898222678,{"$f":"F3358*(1-Elteq!$F$9)","v":4.6390623898222678},""]
["TECHNIK","PA 02/6.40 \"L1\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 6mm, s potiskem \"L1\", žlutá","100ks",2.5607624391818922,{"$f":"F3359*(1-Elteq!$F$9)","v":2.5607624391818922},""]
["TECHNIK","PA 02/6.40 \"L2\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 6mm, s potiskem \"L2\", žlutá","100ks",2.5607624391818922,{"$f":"F3360*(1-Elteq!$F$9)","v":2.5607624391818922},""]
["TECHNIK","PA 02/6.40 \"L3\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 6mm, s potiskem \"L3\", žlutá","100ks",2.5607624391818922,{"$f":"F3361*(1-Elteq!$F$9)","v":2.5607624391818922},""]
["TECHNIK","PA 02/6.40 \"MP\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 6mm, s potiskem \"MP\", žlutá","100ks",2.5607624391818922,{"$f":"F3362*(1-Elteq!$F$9)","v":2.5607624391818922},""]
["TECHNIK","PA 02/6.40 \"PE\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 6mm, s potiskem \"PE\", žlutá","100ks",2.5607624391818922,{"$f":"F3363*(1-Elteq!$F$9)","v":2.5607624391818922},""]
["TECHNIK","PA 02/6.40 \"U1\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 6mm, s potiskem \"U1\", žlutá","100ks",4.6390623898222678,{"$f":"F3364*(1-Elteq!$F$9)","v":4.6390623898222678},""]
["TECHNIK","PA 02/6.40 \"U2\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 6mm, s potiskem \"U2\", žlutá","100ks",4.6390623898222678,{"$f":"F3365*(1-Elteq!$F$9)","v":4.6390623898222678},""]
["TECHNIK","PA 02/6.40 \"V1\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 6mm, s potiskem \"V1\", žlutá","100ks",4.6390623898222678,{"$f":"F3366*(1-Elteq!$F$9)","v":4.6390623898222678},""]
["TECHNIK","PA 02/6.40 \"V2\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 6mm, s potiskem \"V2\", žlutá","100ks",4.6390623898222678,{"$f":"F3367*(1-Elteq!$F$9)","v":4.6390623898222678},""]
["TECHNIK","PA 02/6.40 \"W1\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 6mm, s potiskem \"W1\", žlutá","100ks",4.6390623898222678,{"$f":"F3368*(1-Elteq!$F$9)","v":4.6390623898222678},""]
["TECHNIK","PA 02/6.40 \"W2\"",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 6mm, s potiskem \"W2\", žlutá","100ks",4.6390623898222678,{"$f":"F3369*(1-Elteq!$F$9)","v":4.6390623898222678},""]
["TECHNIK","PA 02/9",null,"Návlečka na vodič, průřez 0,2-1,5mm2 / délka 9mm, bez potisku, žlutá","1000ks",46.761748889408466,{"$f":"F3370*(1-Elteq!$F$9)","v":46.761748889408466},""]
["TECHNIK","PA 1/12",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 12mm, bez potisku, žlutá","100ks",5.0844123792452063,{"$f":"F3371*(1-Elteq!$F$9)","v":5.0844123792452063},""]
["TECHNIK","PA 1/18",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 18mm, bez potisku, žlutá","100ks",7.5709498201899414,{"$f":"F3372*(1-Elteq!$F$9)","v":7.5709498201899414},""]
["TECHNIK","PA 1/21",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 21mm, bez potisku, žlutá","100ks",7.5709498201899414,{"$f":"F3373*(1-Elteq!$F$9)","v":7.5709498201899414},""]
["TECHNIK","PA 1/3",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, bez potisku, žlutá","200ks",3.265899922434877,{"$f":"F3374*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3 euro 0-9",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"0-9\", EURO kódy","200ks",6.1977873528025507,{"$f":"F3375*(1-Elteq!$F$9)","v":6.1977873528025507},"8591735040369"]
["TECHNIK","PA 1/3 žlutá 0-9",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"0-9\", žlutá","200ks",6.1977873528025507,{"$f":"F3376*(1-Elteq!$F$9)","v":6.1977873528025507},"8591735040376"]
["TECHNIK","PA 1/3.09 \"0\"euro",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"0\", černá","200ks",3.265899922434877,{"$f":"F3377*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.1 hnědá",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 6mm, bez potisku, hnědá (cívka)","500ks",10.465724751439037,{"$f":"F3378*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 1/3.19 \"1\"euro",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"1\", hnědá","200ks",3.265899922434877,{"$f":"F3379*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.29 \"+\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"+\", červená","200ks",3.265899922434877,{"$f":"F3380*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.29 \"+\" 1000",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"+\", červená (cívka)","1000ks",16.626399605123009,{"$f":"F3381*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 1/3.29 \"0\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"0\", červená","200ks",3.265899922434877,{"$f":"F3382*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.29 \"1\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"1\", červená","200ks",3.265899922434877,{"$f":"F3383*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.29 \"2\"euro",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"2\", červená","200ks",3.265899922434877,{"$f":"F3384*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.29 \"3\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"3\", červená","200ks",3.265899922434877,{"$f":"F3385*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.29 \"4\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"4\", červená","200ks",3.265899922434877,{"$f":"F3386*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.29 \"5\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"5\", červená","200ks",3.265899922434877,{"$f":"F3387*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.29 \"6\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"6\", červená","200ks",3.265899922434877,{"$f":"F3388*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.29 \"7\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"7\", červená","200ks",3.265899922434877,{"$f":"F3389*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.29 \"8\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"8\", červená","200ks",3.265899922434877,{"$f":"F3390*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.29 \"9\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"9\", červená","200ks",3.265899922434877,{"$f":"F3391*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.30 \"3\"euro",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"3\", oranžová","200ks",3.265899922434877,{"$f":"F3392*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.4. 500",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, bez potisku, žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3393*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 1/3.40 \"-\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"-\", žlutá","200ks",3.265899922434877,{"$f":"F3394*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"-\" 500",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"-\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3395*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 1/3.40 \".\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \".\", žlutá","200ks",3.265899922434877,{"$f":"F3396*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"/\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"/\", žlutá","200ks",3.265899922434877,{"$f":"F3397*(1-Elteq!$F$9)","v":3.265899922434877},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"PA 1/3.40 \"+\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"+\", žlutá","200ks",3.265899922434877,{"$f":"F3398*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"+\" 500",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"+\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3399*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 1/3.40 \"0\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"0\", žlutá","200ks",3.265899922434877,{"$f":"F3400*(1-Elteq!$F$9)","v":3.265899922434877},"7330417001707"]
["TECHNIK","PA 1/3.40 \"0\" 1000",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"0\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3401*(1-Elteq!$F$9)","v":16.626399605123009},"8591735018382"]
["TECHNIK","PA 1/3.40 \"0\" 500",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"0\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3402*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 1/3.40 \"1\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"1\", žlutá","200ks",3.265899922434877,{"$f":"F3403*(1-Elteq!$F$9)","v":3.265899922434877},"7330417001714"]
["TECHNIK","PA 1/3.40 \"1\" 1000",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"1\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3404*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 1/3.40 \"1\" 500",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"1\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3405*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 1/3.40 \"2\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"2\", žlutá","200ks",3.265899922434877,{"$f":"F3406*(1-Elteq!$F$9)","v":3.265899922434877},"7330417001721"]
["TECHNIK","PA 1/3.40 \"2\" 1000",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"2\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3407*(1-Elteq!$F$9)","v":16.626399605123009},"8591735018207"]
["TECHNIK","PA 1/3.40 \"2\" 500",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"2\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3408*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 1/3.40 \"3\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"3\", žlutá","200ks",3.265899922434877,{"$f":"F3409*(1-Elteq!$F$9)","v":3.265899922434877},"7330417001738"]
["TECHNIK","PA 1/3.40 \"3\" 1000",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"3\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3410*(1-Elteq!$F$9)","v":16.626399605123009},"8591735018214"]
["TECHNIK","PA 1/3.40 \"3\" 500",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"3\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3411*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 1/3.40 \"4\" 1000",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"4\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3412*(1-Elteq!$F$9)","v":16.626399605123009},"8591735018368"]
["TECHNIK","PA 1/3.40 \"4\" 500",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"4\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3413*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 1/3.40 \"4\"euro",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"4\", žlutá","200ks",3.265899922434877,{"$f":"F3414*(1-Elteq!$F$9)","v":3.265899922434877},"7330417001745"]
["TECHNIK","PA 1/3.40 \"5\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"5\", žlutá","200ks",3.265899922434877,{"$f":"F3415*(1-Elteq!$F$9)","v":3.265899922434877},"7330417001752"]
["TECHNIK","PA 1/3.40 \"5\" 1000",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"5\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3416*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 1/3.40 \"5\" 500",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"5\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3417*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 1/3.40 \"6\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"6\", žlutá","200ks",3.265899922434877,{"$f":"F3418*(1-Elteq!$F$9)","v":3.265899922434877},"7330417001769"]
["TECHNIK","PA 1/3.40 \"6\" 1000",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"6\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3419*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 1/3.40 \"6\" 500",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"6\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3420*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 1/3.40 \"7\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"7\", žlutá","200ks",3.265899922434877,{"$f":"F3421*(1-Elteq!$F$9)","v":3.265899922434877},"7330417001776"]
["TECHNIK","PA 1/3.40 \"7\" 1000",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"7\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3422*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 1/3.40 \"7\" 500",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"7\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3423*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 1/3.40 \"8\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"8\", žlutá","200ks",3.265899922434877,{"$f":"F3424*(1-Elteq!$F$9)","v":3.265899922434877},"7330417001783"]
["TECHNIK","PA 1/3.40 \"8\" 1000",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"8\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3425*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 1/3.40 \"8\" 500",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"8\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3426*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 1/3.40 \"9\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"9\", žlutá","200ks",3.265899922434877,{"$f":"F3427*(1-Elteq!$F$9)","v":3.265899922434877},"7330417001790"]
["TECHNIK","PA 1/3.40 \"9\" 1000",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"9\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3428*(1-Elteq!$F$9)","v":16.626399605123009},"8591735018375"]
["TECHNIK","PA 1/3.40 \"9\" 500",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"9\", žlutá (cívka)","500ks",10.465724751439037,{"$f":"F3429*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 1/3.40 \"A\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"A\", žlutá","200ks",3.265899922434877,{"$f":"F3430*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"a\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"a\", žlutá","200ks",3.4885749171463458,{"$f":"F3431*(1-Elteq!$F$9)","v":3.4885749171463458},""]
["TECHNIK","PA 1/3.40 \"B\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"B\", žlutá","200ks",3.265899922434877,{"$f":"F3432*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"C\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"C\", žlutá","200ks",3.265899922434877,{"$f":"F3433*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"D\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"D\", žlutá","200ks",3.265899922434877,{"$f":"F3434*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"d\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"d\", žlutá","200ks",3.4885749171463458,{"$f":"F3435*(1-Elteq!$F$9)","v":3.4885749171463458},""]
["TECHNIK","PA 1/3.40 \"E\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"E\", žlutá","200ks",3.265899922434877,{"$f":"F3436*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"e\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"e\", žlutá","200ks",3.4885749171463458,{"$f":"F3437*(1-Elteq!$F$9)","v":3.4885749171463458},""]
["TECHNIK","PA 1/3.40 \"F\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"F\", žlutá","200ks",3.265899922434877,{"$f":"F3438*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"f\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"f\", žlutá","200ks",3.4885749171463458,{"$f":"F3439*(1-Elteq!$F$9)","v":3.4885749171463458},""]
["TECHNIK","PA 1/3.40 \"G\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"G\", žlutá","200ks",3.265899922434877,{"$f":"F3440*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"H\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"H\", žlutá","200ks",3.265899922434877,{"$f":"F3441*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"I\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"I\", žlutá","200ks",3.265899922434877,{"$f":"F3442*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"J\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"J\", žlutá","200ks",3.265899922434877,{"$f":"F3443*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"K\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"K\", žlutá","200ks",3.265899922434877,{"$f":"F3444*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"k\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"k\", žlutá","200ks",3.4885749171463458,{"$f":"F3445*(1-Elteq!$F$9)","v":3.4885749171463458},""]
["TECHNIK","PA 1/3.40 \"L\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"L\", žlutá","200ks",3.265899922434877,{"$f":"F3446*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"l\" malé L",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"l\", žlutá (malé L)","200ks",3.4885749171463458,{"$f":"F3447*(1-Elteq!$F$9)","v":3.4885749171463458},""]
["TECHNIK","PA 1/3.40 \"M\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"M\", žlutá","200ks",3.265899922434877,{"$f":"F3448*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"N\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"N\", žlutá","200ks",3.265899922434877,{"$f":"F3449*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"n\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"n\", žlutá","200ks",3.4885749171463458,{"$f":"F3450*(1-Elteq!$F$9)","v":3.4885749171463458},""]
["TECHNIK","PA 1/3.40 \"N\" 1000",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"N\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3451*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 1/3.40 \"P\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"P\", žlutá","200ks",3.265899922434877,{"$f":"F3452*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"Q\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"Q\", žlutá","200ks",3.265899922434877,{"$f":"F3453*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"R\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"R\", žlutá","200ks",3.265899922434877,{"$f":"F3454*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"r\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"r\", žlutá","200ks",3.4885749171463458,{"$f":"F3455*(1-Elteq!$F$9)","v":3.4885749171463458},""]
["TECHNIK","PA 1/3.40 \"S\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"S\", žlutá","200ks",3.265899922434877,{"$f":"F3456*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"T\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"T\", žlutá","200ks",3.265899922434877,{"$f":"F3457*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"U\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"U\", žlutá","200ks",3.265899922434877,{"$f":"F3458*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"U\" 1000",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"U\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3459*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 1/3.40 \"V\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"V\", žlutá","200ks",3.265899922434877,{"$f":"F3460*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"V\" 1000",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"V\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3461*(1-Elteq!$F$9)","v":16.626399605123009},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"PA 1/3.40 \"W\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"W\", žlutá","200ks",3.265899922434877,{"$f":"F3462*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"W\" 1000",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"W\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3463*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 1/3.40 \"X\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"X\", žlutá","200ks",3.265899922434877,{"$f":"F3464*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"Y\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"Y\", žlutá","200ks",3.265899922434877,{"$f":"F3465*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"Z\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"Z\", žlutá","200ks",3.265899922434877,{"$f":"F3466*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"zem\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"zem\", žlutá","200ks",3.265899922434877,{"$f":"F3467*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.40 \"zem\" 1000",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"zem\", žlutá (cívka)","1000ks",16.626399605123009,{"$f":"F3468*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 1/3.59 \"5\"euro",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"5\", zelená","200ks",3.265899922434877,{"$f":"F3469*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.6 modrá",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, bez potisku, modrá (cívka)","500ks",10.465724751439037,{"$f":"F3470*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 1/3.69 \"-\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"-\", modrá","200ks",3.265899922434877,{"$f":"F3471*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.69 \"-\" 1000",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"-\", modrá (cívka)","1000ks",16.626399605123009,{"$f":"F3472*(1-Elteq!$F$9)","v":16.626399605123009},""]
["TECHNIK","PA 1/3.69 \"0\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"0\", modrá","200ks",3.265899922434877,{"$f":"F3473*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.69 \"1\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"1\", modrá","200ks",3.265899922434877,{"$f":"F3474*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.69 \"2\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"2\", modrá","200ks",3.265899922434877,{"$f":"F3475*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.69 \"3\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"3\", modrá","200ks",3.265899922434877,{"$f":"F3476*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.69 \"4\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"4\", modrá","200ks",3.265899922434877,{"$f":"F3477*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.69 \"5\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"5\", modrá","200ks",3.265899922434877,{"$f":"F3478*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.69 \"6\"euro",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"6\", modrá","200ks",3.265899922434877,{"$f":"F3479*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.69 \"7\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"7\", modrá","200ks",3.265899922434877,{"$f":"F3480*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.69 \"8\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"8\", modrá","200ks",3.265899922434877,{"$f":"F3481*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.69 \"9\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"9\", modrá","200ks",3.265899922434877,{"$f":"F3482*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.79 \"7\"euro",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"7\", fialová","200ks",3.265899922434877,{"$f":"F3483*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.8 šedá",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, bez potisku, šedá (cívka)","500ks",10.465724751439037,{"$f":"F3484*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PA 1/3.80 \"8\"euro",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"8\", šedá","200ks",3.265899922434877,{"$f":"F3485*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.90 \"1\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"1\", bílá","200ks",3.265899922434877,{"$f":"F3486*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.90 \"2\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"2\", bílá","200ks",3.265899922434877,{"$f":"F3487*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.90 \"3\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"3\", bílá","200ks",3.265899922434877,{"$f":"F3488*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.90 \"4\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"4\", bílá","200ks",3.265899922434877,{"$f":"F3489*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.90 \"5\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"5\", bílá","200ks",3.265899922434877,{"$f":"F3490*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.90 \"6\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"6\", bílá","200ks",3.265899922434877,{"$f":"F3491*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.90 \"7\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"7\", bílá","200ks",3.265899922434877,{"$f":"F3492*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.90 \"8\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"8\", bílá","200ks",3.265899922434877,{"$f":"F3493*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/3.90 \"9\"euro",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 3mm, s potiskem \"9\", bílá","200ks",3.265899922434877,{"$f":"F3494*(1-Elteq!$F$9)","v":3.265899922434877},""]
["TECHNIK","PA 1/6",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 6mm, bez potisku, žlutá","100ks",4.6390623898222678,{"$f":"F3495*(1-Elteq!$F$9)","v":4.6390623898222678},""]
["TECHNIK","PA 1/6.40 \"L1\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 6mm, s potiskem \"L1\", žlutá","100ks",2.5607624391818922,{"$f":"F3496*(1-Elteq!$F$9)","v":2.5607624391818922},""]
["TECHNIK","PA 1/6.40 \"L1\" 1000",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 6mm, s potiskem \"L1\", žlutá (cívka)","1000ks",25.60762439181892,{"$f":"F3497*(1-Elteq!$F$9)","v":25.60762439181892},""]
["TECHNIK","PA 1/6.40 \"L2\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 6mm, s potiskem \"L2\", žlutá","100ks",2.5607624391818922,{"$f":"F3498*(1-Elteq!$F$9)","v":2.5607624391818922},""]
["TECHNIK","PA 1/6.40 \"L2\" 1000",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 6mm, s potiskem \"L2\", žlutá (cívka)","1000ks",25.60762439181892,{"$f":"F3499*(1-Elteq!$F$9)","v":25.60762439181892},""]
["TECHNIK","PA 1/6.40 \"L3\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 6mm, s potiskem \"L3\", žlutá","100ks",2.5607624391818922,{"$f":"F3500*(1-Elteq!$F$9)","v":2.5607624391818922},""]
["TECHNIK","PA 1/6.40 \"L3\" 1000",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 6mm, s potiskem \"L3\", žlutá (cívka)","1000ks",25.60762439181892,{"$f":"F3501*(1-Elteq!$F$9)","v":25.60762439181892},""]
["TECHNIK","PA 1/6.40 \"MP\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 6mm, s potiskem \"MP\", žlutá","100ks",2.5607624391818922,{"$f":"F3502*(1-Elteq!$F$9)","v":2.5607624391818922},""]
["TECHNIK","PA 1/6.40 \"PE\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 6mm, s potiskem \"PE\", žlutá","100ks",2.5607624391818922,{"$f":"F3503*(1-Elteq!$F$9)","v":2.5607624391818922},""]
["TECHNIK","PA 1/6.40 \"U1\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 6mm, s potiskem \"U1\", žlutá","100ks",4.6390623898222678,{"$f":"F3504*(1-Elteq!$F$9)","v":4.6390623898222678},""]
["TECHNIK","PA 1/6.40 \"U2\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 6mm, s potiskem \"U2\", žlutá","100ks",4.6390623898222678,{"$f":"F3505*(1-Elteq!$F$9)","v":4.6390623898222678},""]
["TECHNIK","PA 1/6.40 \"V1\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 6mm, s potiskem \"V1\", žlutá","100ks",4.6390623898222678,{"$f":"F3506*(1-Elteq!$F$9)","v":4.6390623898222678},""]
["TECHNIK","PA 1/6.40 \"V2\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 6mm, s potiskem \"V2\", žlutá","100ks",4.6390623898222678,{"$f":"F3507*(1-Elteq!$F$9)","v":4.6390623898222678},""]
["TECHNIK","PA 1/6.40 \"W1\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 6mm, s potiskem \"W1\", žlutá","100ks",4.6390623898222678,{"$f":"F3508*(1-Elteq!$F$9)","v":4.6390623898222678},""]
["TECHNIK","PA 1/6.40 \"W2\"",null,"Návlečka na vodič, průřez 1,5-4,0mm2 / délka 6mm, s potiskem \"W2\", žlutá","100ks",4.6390623898222678,{"$f":"F3509*(1-Elteq!$F$9)","v":4.6390623898222678},""]
["TECHNIK","PA 2/12",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 12mm, bez potisku, žlutá","100ks",6.8658123369369566,{"$f":"F3510*(1-Elteq!$F$9)","v":6.8658123369369566},""]
["TECHNIK","PA 2/4",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, bez potisku, žlutá","100ks",2.8947749312490956,{"$f":"F3511*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.19 \"1\"euro",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"1\", hnědá","100ks",2.8947749312490956,{"$f":"F3512*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.29 \"0\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"0\", červená","100ks",2.8947749312490956,{"$f":"F3513*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.29 \"1\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"1\", červená","100ks",2.8947749312490956,{"$f":"F3514*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.29 \"2\"euro",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"2\", červená","100ks",2.8947749312490956,{"$f":"F3515*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.29 \"3\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"3\", červená","100ks",2.8947749312490956,{"$f":"F3516*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.29 \"4\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"4\", červená","100ks",2.8947749312490956,{"$f":"F3517*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.29 \"5\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"5\", červená","100ks",2.8947749312490956,{"$f":"F3518*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.29 \"6\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"6\", červená","100ks",2.8947749312490956,{"$f":"F3519*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.29 \"7\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"7\", červená","100ks",2.8947749312490956,{"$f":"F3520*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.29 \"8\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"8\", červená","100ks",2.8947749312490956,{"$f":"F3521*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.29 \"9\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"9\", červená","100ks",2.8947749312490956,{"$f":"F3522*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"+\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"+\", žlutá","100ks",2.8947749312490956,{"$f":"F3523*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"0\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"0\", žlutá","100ks",2.8947749312490956,{"$f":"F3524*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"0\" 250",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"0\", žlutá (cívka)","250ks",7.19982482900416,{"$f":"F3525*(1-Elteq!$F$9)","v":7.19982482900416},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"PA 2/4.40 \"1\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"1\", žlutá","100ks",2.8947749312490956,{"$f":"F3526*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"1\" 250",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"1\", žlutá (cívka)","250ks",7.19982482900416,{"$f":"F3527*(1-Elteq!$F$9)","v":7.19982482900416},""]
["TECHNIK","PA 2/4.40 \"2\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"2\", žlutá","100ks",2.8947749312490956,{"$f":"F3528*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"2\" 250",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"2\", žlutá (cívka)","250ks",7.19982482900416,{"$f":"F3529*(1-Elteq!$F$9)","v":7.19982482900416},""]
["TECHNIK","PA 2/4.40 \"3\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"3\", žlutá","100ks",2.8947749312490956,{"$f":"F3530*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"3\" 250",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"3\", žlutá (cívka)","250ks",7.19982482900416,{"$f":"F3531*(1-Elteq!$F$9)","v":7.19982482900416},""]
["TECHNIK","PA 2/4.40 \"4\"euro",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"4\", žlutá","100ks",2.8947749312490956,{"$f":"F3532*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"4\"euro250",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"4\", žlutá (cívka)","250ks",7.19982482900416,{"$f":"F3533*(1-Elteq!$F$9)","v":7.19982482900416},""]
["TECHNIK","PA 2/4.40 \"5\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"5\", žlutá","100ks",2.8947749312490956,{"$f":"F3534*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"5\" 250",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"5\", žlutá (cívka)","250ks",7.19982482900416,{"$f":"F3535*(1-Elteq!$F$9)","v":7.19982482900416},""]
["TECHNIK","PA 2/4.40 \"6\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"6\", žlutá","100ks",2.8947749312490956,{"$f":"F3536*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"6\" 250",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"6\", žlutá (cívka)","250ks",7.19982482900416,{"$f":"F3537*(1-Elteq!$F$9)","v":7.19982482900416},""]
["TECHNIK","PA 2/4.40 \"7\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"7\", žlutá","100ks",2.8947749312490956,{"$f":"F3538*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"7\" 250",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"7\", žlutá (cívka)","250ks",7.19982482900416,{"$f":"F3539*(1-Elteq!$F$9)","v":7.19982482900416},""]
["TECHNIK","PA 2/4.40 \"8\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"8\", žlutá","100ks",2.8947749312490956,{"$f":"F3540*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"8\" 250",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"8\", žlutá (cívka)","250ks",7.19982482900416,{"$f":"F3541*(1-Elteq!$F$9)","v":7.19982482900416},""]
["TECHNIK","PA 2/4.40 \"9\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"9\", žlutá","100ks",2.8947749312490956,{"$f":"F3542*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"9\" 250",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"9\", žlutá (cívka)","250ks",7.19982482900416,{"$f":"F3543*(1-Elteq!$F$9)","v":7.19982482900416},""]
["TECHNIK","PA 2/4.40 \"A\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"A\", žlutá","100ks",2.8947749312490956,{"$f":"F3544*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"B\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"B\", žlutá","100ks",2.8947749312490956,{"$f":"F3545*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"C\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"C\", žlutá","100ks",2.8947749312490956,{"$f":"F3546*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"D\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"D\", žlutá","100ks",2.8947749312490956,{"$f":"F3547*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"E\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"E\", žlutá","100ks",2.8947749312490956,{"$f":"F3548*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"F\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"F\", žlutá","100ks",2.8947749312490956,{"$f":"F3549*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"G\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"G\", žlutá","100ks",2.8947749312490956,{"$f":"F3550*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"H\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"H\", žlutá","100ks",2.8947749312490956,{"$f":"F3551*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"I\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"I\", žlutá","100ks",2.8947749312490956,{"$f":"F3552*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"J\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"J\", žlutá","100ks",2.8947749312490956,{"$f":"F3553*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"K\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"K\", žlutá","100ks",2.8947749312490956,{"$f":"F3554*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"L\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"L\", žlutá","100ks",2.8947749312490956,{"$f":"F3555*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"M\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"M\", žlutá","100ks",2.8947749312490956,{"$f":"F3556*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"N\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"N\", žlutá","100ks",2.8947749312490956,{"$f":"F3557*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"O\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"O\", žlutá","100ks",2.8947749312490956,{"$f":"F3558*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"P\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"P\", žlutá","100ks",2.8947749312490956,{"$f":"F3559*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"Q\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"Q\", žlutá","100ks",2.8947749312490956,{"$f":"F3560*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"R\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"R\", žlutá","100ks",2.8947749312490956,{"$f":"F3561*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"S\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"S\", žlutá","100ks",2.8947749312490956,{"$f":"F3562*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"T\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"T\", žlutá","100ks",2.8947749312490956,{"$f":"F3563*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"U\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"U\", žlutá","100ks",2.8947749312490956,{"$f":"F3564*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"V\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"V\", žlutá","100ks",2.8947749312490956,{"$f":"F3565*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"W\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"W\", žlutá","100ks",2.8947749312490956,{"$f":"F3566*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"X\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"X\", žlutá","100ks",2.8947749312490956,{"$f":"F3567*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"Y\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"Y\", žlutá","100ks",2.8947749312490956,{"$f":"F3568*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"Z\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"Z\", žlutá","100ks",2.8947749312490956,{"$f":"F3569*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/4.40 \"zem\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 4mm, s potiskem \"zem\", žlutá","100ks",2.8947749312490956,{"$f":"F3570*(1-Elteq!$F$9)","v":2.8947749312490956},""]
["TECHNIK","PA 2/6",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 6mm, bez potisku, žlutá","100ks",7.7936248149014107,{"$f":"F3571*(1-Elteq!$F$9)","v":7.7936248149014107},""]
["TECHNIK","PA 2/6.40 \"L1\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 6mm, s potiskem \"L1\", žlutá","100ks",4.4163873951107995,{"$f":"F3572*(1-Elteq!$F$9)","v":4.4163873951107995},""]
["TECHNIK","PA 2/6.40 \"L2\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 6mm, s potiskem \"L2\", žlutá","100ks",4.4163873951107995,{"$f":"F3573*(1-Elteq!$F$9)","v":4.4163873951107995},""]
["TECHNIK","PA 2/6.40 \"L3\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 6mm, s potiskem \"L3\", žlutá","100ks",4.4163873951107995,{"$f":"F3574*(1-Elteq!$F$9)","v":4.4163873951107995},""]
["TECHNIK","PA 2/6.40 \"W1\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 6mm, s potiskem \"W1\", žlutá","100ks",7.7936248149014107,{"$f":"F3575*(1-Elteq!$F$9)","v":7.7936248149014107},""]
["TECHNIK","PA 2/9.40 \"XY\"",null,"Návlečka na vodič, průřez 2,5-16mm2 / délka 9mm, s potiskem \"XY\", žlutá (znaky na zakázku)","100ks",11.504874726759224,{"$f":"F3576*(1-Elteq!$F$9)","v":11.504874726759224},""]
["TECHNIK","PA 3/15",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 15mm, bez potisku, žlutá","20ks",3.5627999153835019,{"$f":"F3577*(1-Elteq!$F$9)","v":3.5627999153835019},""]
["TECHNIK","PA 3/18",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 18mm, bez potisku, žlutá","20ks",4.0823749030435961,{"$f":"F3578*(1-Elteq!$F$9)","v":4.0823749030435961},""]
["TECHNIK","PA 3/6",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, bez potisku, žlutá","20ks",1.1690437222352117,{"$f":"F3579*(1-Elteq!$F$9)","v":1.1690437222352117},""]
["TECHNIK","PA 3/6.40 \"0\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"0\", žlutá","20ks",1.1690437222352117,{"$f":"F3580*(1-Elteq!$F$9)","v":1.1690437222352117},""]
["TECHNIK","PA 3/6.40 \"1\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"1\", žlutá","20ks",1.1690437222352117,{"$f":"F3581*(1-Elteq!$F$9)","v":1.1690437222352117},""]
["TECHNIK","PA 3/6.40 \"2\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"2\", žlutá","20ks",1.1690437222352117,{"$f":"F3582*(1-Elteq!$F$9)","v":1.1690437222352117},""]
["TECHNIK","PA 3/6.40 \"3\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"3\", žlutá","20ks",1.1690437222352117,{"$f":"F3583*(1-Elteq!$F$9)","v":1.1690437222352117},""]
["TECHNIK","PA 3/6.40 \"4\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"4\", žlutá","20ks",1.1690437222352117,{"$f":"F3584*(1-Elteq!$F$9)","v":1.1690437222352117},""]
["TECHNIK","PA 3/6.40 \"5\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"5\", žlutá","20ks",1.1690437222352117,{"$f":"F3585*(1-Elteq!$F$9)","v":1.1690437222352117},""]
["TECHNIK","PA 3/6.40 \"6\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"6\", žlutá","20ks",1.1690437222352117,{"$f":"F3586*(1-Elteq!$F$9)","v":1.1690437222352117},""]
["TECHNIK","PA 3/6.40 \"7\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"7\", žlutá","20ks",1.1690437222352117,{"$f":"F3587*(1-Elteq!$F$9)","v":1.1690437222352117},""]
["TECHNIK","PA 3/6.40 \"8\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"8\", žlutá","20ks",1.1690437222352117,{"$f":"F3588*(1-Elteq!$F$9)","v":1.1690437222352117},""]
["TECHNIK","PA 3/6.40 \"9\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"9\", žlutá","20ks",1.1690437222352117,{"$f":"F3589*(1-Elteq!$F$9)","v":1.1690437222352117},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"PA 3/6.40 \"D\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"D\", žlutá","20ks",1.1690437222352117,{"$f":"F3590*(1-Elteq!$F$9)","v":1.1690437222352117},""]
["TECHNIK","PA 3/6.40 \"E\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"E\", žlutá","20ks",1.1690437222352117,{"$f":"F3591*(1-Elteq!$F$9)","v":1.1690437222352117},""]
["TECHNIK","PA 3/6.40 \"H\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"H\", žlutá","20ks",1.1690437222352117,{"$f":"F3592*(1-Elteq!$F$9)","v":1.1690437222352117},""]
["TECHNIK","PA 3/6.40 \"L\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"L\", žlutá","20ks",1.1690437222352117,{"$f":"F3593*(1-Elteq!$F$9)","v":1.1690437222352117},""]
["TECHNIK","PA 3/6.40 \"L1\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"L1\", žlutá","20ks",1.781399957691751,{"$f":"F3594*(1-Elteq!$F$9)","v":1.781399957691751},""]
["TECHNIK","PA 3/6.40 \"L2\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"L2\", žlutá","20ks",1.781399957691751,{"$f":"F3595*(1-Elteq!$F$9)","v":1.781399957691751},""]
["TECHNIK","PA 3/6.40 \"L3\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"L3\", žlutá","20ks",1.781399957691751,{"$f":"F3596*(1-Elteq!$F$9)","v":1.781399957691751},""]
["TECHNIK","PA 3/6.40 \"P\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"P\", žlutá","20ks",1.1690437222352117,{"$f":"F3597*(1-Elteq!$F$9)","v":1.1690437222352117},""]
["TECHNIK","PA 3/6.40 \"PE\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"PE\", žlutá","20ks",1.781399957691751,{"$f":"F3598*(1-Elteq!$F$9)","v":1.781399957691751},""]
["TECHNIK","PA 3/6.40 \"R\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"R\", žlutá","20ks",1.1690437222352117,{"$f":"F3599*(1-Elteq!$F$9)","v":1.1690437222352117},""]
["TECHNIK","PA 3/6.40 \"U\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"U\", žlutá","20ks",1.1690437222352117,{"$f":"F3600*(1-Elteq!$F$9)","v":1.1690437222352117},""]
["TECHNIK","PA 3/6.40 \"V\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"V\", žlutá","20ks",1.1690437222352117,{"$f":"F3601*(1-Elteq!$F$9)","v":1.1690437222352117},""]
["TECHNIK","PA 3/6.40 \"W\"",null,"Návlečka na vodič pro průřez 16-70mm2 / délka 6mm, s potiskem \"W\", žlutá","20ks",1.1690437222352117,{"$f":"F3602*(1-Elteq!$F$9)","v":1.1690437222352117},""]
["TECHNIK","PSK 18000",null,"Plastový box 18-ti dílný pro návlečky - prázdný","1ks",11.875999717945007,{"$f":"F3603*(1-Elteq!$F$9)","v":11.875999717945007},""]
["TECHNIK","PSK 18001",null,"Plastový box 18-ti dílný s návlečkami PA 1","1ks",158.65593373192158,{"$f":"F3604*(1-Elteq!$F$9)","v":158.65593373192158},""]
["TECHNIK","PSK 18002",null,"Plastový box 18-ti dílný s návlečkami PA 02","1ks",95.193560239152944,{"$f":"F3605*(1-Elteq!$F$9)","v":95.193560239152944},""]
["TECHNIK","PC 10/12",null,"Návlečka žlutá pro průřez 0,4-1,5mm2 / délka 12mm, bez potisku","100ks",4.824624885415159,{"$f":"F3606*(1-Elteq!$F$9)","v":4.824624885415159},"8591735017149"]
["TECHNIK","PC 10/15",null,"Návlečka žlutá pro průřez 0,4-1,5mm2 / délka 15mm, bez potisku","100ks",7.979187310494301,{"$f":"F3607*(1-Elteq!$F$9)","v":7.979187310494301},""]
["TECHNIK","PC 10/3",null,"Návlečka žlutá pro průřez 0,4-1,5mm2 / délka 3mm, bez potisku","200ks",4.2679373986364864,{"$f":"F3608*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 10/3 \"0\"",null,"Návlečka žlutá pro průřez 0,4-1,5mm2 / délka 3mm, s potiskem \"0\"","200ks",4.2679373986364864,{"$f":"F3609*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 10/3 \"1\"",null,"Návlečka žlutá pro průřez 0,4-1,5mm2 / délka 3mm, s potiskem \"1\"","200ks",4.2679373986364864,{"$f":"F3610*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 10/3 \"2\"",null,"Návlečka žlutá pro průřez 0,4-1,5mm2 / délka 3mm, s potiskem \"2\"","200ks",4.2679373986364864,{"$f":"F3611*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 10/3 \"3\"",null,"Návlečka žlutá pro průřez 0,4-1,5mm2 / délka 3mm, s potiskem \"3\"","200ks",4.2679373986364864,{"$f":"F3612*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 10/3 \"4\"",null,"Návlečka žlutá pro průřez 0,4-1,5mm2 / délka 3mm, s potiskem \"4\"","200ks",4.2679373986364864,{"$f":"F3613*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 10/3 \"5\"",null,"Návlečka žlutá pro průřez 0,4-1,5mm2 / délka 3mm, s potiskem \"5\"","200ks",4.2679373986364864,{"$f":"F3614*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 10/3 \"6\"",null,"Návlečka žlutá pro průřez 0,4-1,5mm2 / délka 3mm, s potiskem \"6\"","200ks",4.2679373986364864,{"$f":"F3615*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 10/3 \"7\"",null,"Návlečka žlutá pro průřez 0,4-1,5mm2 / délka 3mm, s potiskem \"7\"","200ks",4.2679373986364864,{"$f":"F3616*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 10/3 \"8\"",null,"Návlečka žlutá pro průřez 0,4-1,5mm2 / délka 3mm, s potiskem \"8\"","200ks",4.2679373986364864,{"$f":"F3617*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 10/3 \"9\"",null,"Návlečka žlutá pro průřez 0,4-1,5mm2 / délka 3mm, s potiskem \"9\"","200ks",4.2679373986364864,{"$f":"F3618*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 10/3 \"A\"",null,"Návlečka žlutá pro průřez 0,4-1,5mm2 / délka 3mm, s potiskem \"A\"","200ks",4.2679373986364864,{"$f":"F3619*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 10/3 \"L\"",null,"Návlečka žlutá pro průřez 0,4-1,5mm2 / délka 3mm, s potiskem \"L\"","200ks",4.2679373986364864,{"$f":"F3620*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 10/3 \"X\"",null,"Návlečka žlutá pro průřez 0,4-1,5mm2 / délka 3mm, s potiskem \"X\"","200ks",4.2679373986364864,{"$f":"F3621*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 20/12",null,"Návlečka žlutá pro průřez 1,5-3,0mm2 / délka 12mm, bez potisku","100ks",5.7524373633796122,{"$f":"F3622*(1-Elteq!$F$9)","v":5.7524373633796122},""]
["TECHNIK","PC 20/21",null,"Návlečka žlutá pro průřez 1,5-3,0mm2 / délka 21mm, bez potisku","100ks",7.8307373140199887,{"$f":"F3623*(1-Elteq!$F$9)","v":7.8307373140199887},""]
["TECHNIK","PC 20/3",null,"Návlečka žlutá pro průřez 1,5-3,0mm2 / délka 3mm, bez potisku","200ks",4.2679373986364864,{"$f":"F3624*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 20/3 \"0\"",null,"Návlečka žlutá pro průřez 1,5-3,0mm2 / délka 3mm, s potiskem \"0\"","200ks",4.2679373986364864,{"$f":"F3625*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 20/3 \"1\"",null,"Návlečka žlutá pro průřez 1,5-3,0mm2 / délka 3mm, s potiskem \"1\"","200ks",4.2679373986364864,{"$f":"F3626*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 20/3 \"2\"",null,"Návlečka žlutá pro průřez 1,5-3,0mm2 / délka 3mm, s potiskem \"2\"","200ks",4.2679373986364864,{"$f":"F3627*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 20/3 \"3\"",null,"Návlečka žlutá pro průřez 1,5-3,0mm2 / délka 3mm, s potiskem \"3\"","200ks",4.2679373986364864,{"$f":"F3628*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 20/3 \"4\"",null,"Návlečka žlutá pro průřez 1,5-3,0mm2 / délka 3mm, s potiskem \"4\"","200ks",4.2679373986364864,{"$f":"F3629*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 20/3 \"5\"",null,"Návlečka žlutá pro průřez 1,5-3,0mm2 / délka 3mm, s potiskem \"5\"","200ks",4.2679373986364864,{"$f":"F3630*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 20/3 \"6\"",null,"Návlečka žlutá pro průřez 1,5-3,0mm2 / délka 3mm, s potiskem \"6\"","200ks",4.2679373986364864,{"$f":"F3631*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 20/3 \"7\"",null,"Návlečka žlutá pro průřez 1,5-3,0mm2 / délka 3mm, s potiskem \"7\"","200ks",4.2679373986364864,{"$f":"F3632*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 20/3 \"8\"",null,"Návlečka žlutá pro průřez 1,5-3,0mm2 / délka 3mm, s potiskem \"8\"","200ks",4.2679373986364864,{"$f":"F3633*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 20/3 \"9\"",null,"Návlečka žlutá pro průřez 1,5-3,0mm2 / délka 3mm, s potiskem \"9\"","200ks",4.2679373986364864,{"$f":"F3634*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 20/6 \"L1\"",null,"Návlečka žlutá pro průřez 1,5-3,0mm2 / délka 3mm, s potiskem \"L1\"","100ks",3.1916749241977205,{"$f":"F3635*(1-Elteq!$F$9)","v":3.1916749241977205},""]
["TECHNIK","PC 20/6 \"L2\"",null,"Návlečka žlutá pro průřez 1,5-3,0mm2 / délka 3mm, s potiskem \"L2\"","100ks",3.1916749241977205,{"$f":"F3636*(1-Elteq!$F$9)","v":3.1916749241977205},""]
["TECHNIK","PC 20/6 \"L3\"",null,"Návlečka žlutá pro průřez 1,5-3,0mm2 / délka 3mm, s potiskem \"L3\"","100ks",3.1916749241977205,{"$f":"F3637*(1-Elteq!$F$9)","v":3.1916749241977205},""]
["TECHNIK","PC 30/12",null,"Návlečka žlutá pro průřez 3,0-4,0mm2 / délka 12mm, bez potisku","100ks",5.5668748677867219,{"$f":"F3638*(1-Elteq!$F$9)","v":5.5668748677867219},""]
["TECHNIK","PC 30/3",null,"Návlečka žlutá pro průřez 3,0-4,0mm2 / délka 3mm, bez potisku","200ks",4.2679373986364864,{"$f":"F3639*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 30/3 \"0\"",null,"Návlečka žlutá pro průřez 3,0-4,0mm2 / délka 3mm, s potiskem \"0\"","200ks",4.2679373986364864,{"$f":"F3640*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 30/3 \"1\"",null,"Návlečka žlutá pro průřez 3,0-4,0mm2 / délka 3mm, s potiskem \"1\"","200ks",4.2679373986364864,{"$f":"F3641*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 30/3 \"2\"",null,"Návlečka žlutá pro průřez 3,0-4,0mm2 / délka 3mm, s potiskem \"2\"","200ks",4.2679373986364864,{"$f":"F3642*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 30/3 \"3\"",null,"Návlečka žlutá pro průřez 3,0-4,0mm2 / délka 3mm, s potiskem \"3\"","200ks",4.2679373986364864,{"$f":"F3643*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 30/3 \"4\"",null,"Návlečka žlutá pro průřez 3,0-4,0mm2 / délka 3mm, s potiskem \"4\"","200ks",4.2679373986364864,{"$f":"F3644*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 30/3 \"5\"",null,"Návlečka žlutá pro průřez 3,0-4,0mm2 / délka 3mm, s potiskem \"5\"","200ks",4.2679373986364864,{"$f":"F3645*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 30/3 \"6\"",null,"Návlečka žlutá pro průřez 3,0-4,0mm2 / délka 3mm, s potiskem \"6\"","200ks",4.2679373986364864,{"$f":"F3646*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 30/3 \"7\"",null,"Návlečka žlutá pro průřez 3,0-4,0mm2 / délka 3mm, s potiskem \"7\"","200ks",4.2679373986364864,{"$f":"F3647*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 30/3 \"8\"",null,"Návlečka žlutá pro průřez 3,0-4,0mm2 / délka 3mm, s potiskem \"8\"","200ks",4.2679373986364864,{"$f":"F3648*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 30/3 \"9\"",null,"Návlečka žlutá pro průřez 3,0-4,0mm2 / délka 3mm, s potiskem \"9\"","200ks",4.2679373986364864,{"$f":"F3649*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","PC 30/6",null,"Návlečka žlutá pro průřez 3,0-4,0mm2 / délka 6mm, bez potisku","100ks",5.5668748677867219,{"$f":"F3650*(1-Elteq!$F$9)","v":5.5668748677867219},""]
["TECHNIK","PC 40/12.",null,"Návlečka žlutá pro průřez 4,0-5,0mm2 / délka 12mm, bez potisku","100ks",10.465724751439037,{"$f":"F3651*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PC 40/15",null,"Návlečka žlutá pro průřez 4,0-5,0mm2 / délka 15mm, bez potisku","100ks",10.465724751439037,{"$f":"F3652*(1-Elteq!$F$9)","v":10.465724751439037},""]
["TECHNIK","PC 40/21",null,"Návlečka žlutá pro průřez 4,0-5,0mm2 / délka 21mm, bez potisku","100ks",10.465724751439037,{"$f":"F3653*(1-Elteq!$F$9)","v":10.465724751439037},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"PC 40/4",null,"Návlečka žlutá pro průřez 4,0-5,0mm2 / délka 4mm, bez potisku","200ks",4.5277248924665336,{"$f":"F3654*(1-Elteq!$F$9)","v":4.5277248924665336},""]
["TECHNIK","PC 40/4 \"0\"",null,"Návlečka žlutá pro průřez 4,0-5,0mm2 / délka 4mm, s potiskem \"0\"","200ks",4.5277248924665336,{"$f":"F3655*(1-Elteq!$F$9)","v":4.5277248924665336},""]
["TECHNIK","PC 40/4 \"1\"",null,"Návlečka žlutá pro průřez 4,0-5,0mm2 / délka 4mm, s potiskem \"1\"","200ks",4.5277248924665336,{"$f":"F3656*(1-Elteq!$F$9)","v":4.5277248924665336},""]
["TECHNIK","PC 40/4 \"2\"",null,"Návlečka žlutá pro průřez 4,0-5,0mm2 / délka 4mm, s potiskem \"2\"","200ks",4.5277248924665336,{"$f":"F3657*(1-Elteq!$F$9)","v":4.5277248924665336},""]
["TECHNIK","PC 40/4 \"3\"",null,"Návlečka žlutá pro průřez 4,0-5,0mm2 / délka 4mm, s potiskem \"3\"","200ks",4.5277248924665336,{"$f":"F3658*(1-Elteq!$F$9)","v":4.5277248924665336},""]
["TECHNIK","PC 40/4 \"4\"",null,"Návlečka žlutá pro průřez 4,0-5,0mm2 / délka 4mm, s potiskem \"4\"","200ks",4.5277248924665336,{"$f":"F3659*(1-Elteq!$F$9)","v":4.5277248924665336},""]
["TECHNIK","PC 40/4 \"5\"",null,"Návlečka žlutá pro průřez 4,0-5,0mm2 / délka 4mm, s potiskem \"5\"","200ks",4.5277248924665336,{"$f":"F3660*(1-Elteq!$F$9)","v":4.5277248924665336},""]
["TECHNIK","PC 40/4 \"6\"",null,"Návlečka žlutá pro průřez 4,0-5,0mm2 / délka 4mm, s potiskem \"6\"","200ks",4.5277248924665336,{"$f":"F3661*(1-Elteq!$F$9)","v":4.5277248924665336},""]
["TECHNIK","PC 40/4 \"7\"",null,"Návlečka žlutá pro průřez 4,0-5,0mm2 / délka 4mm, s potiskem \"7\"","200ks",4.5277248924665336,{"$f":"F3662*(1-Elteq!$F$9)","v":4.5277248924665336},""]
["TECHNIK","PC 40/4 \"8\"",null,"Návlečka žlutá pro průřez 4,0-5,0mm2 / délka 4mm, s potiskem \"8\"","200ks",4.5277248924665336,{"$f":"F3663*(1-Elteq!$F$9)","v":4.5277248924665336},""]
["TECHNIK","PC 40/4 \"9\"",null,"Návlečka žlutá pro průřez 4,0-5,0mm2 / délka 4mm, s potiskem \"9\"","200ks",4.5277248924665336,{"$f":"F3664*(1-Elteq!$F$9)","v":4.5277248924665336},""]
["TECHNIK","PC 40/4 \"A\"",null,"Návlečka žlutá pro průřez 4,0-5,0mm2 / délka 4mm, s potiskem \"A\"","200ks",4.5277248924665336,{"$f":"F3665*(1-Elteq!$F$9)","v":4.5277248924665336},""]
["TECHNIK","PC 40/4 \"B\"",null,"Návlečka žlutá pro průřez 4,0-5,0mm2 / délka 4mm, s potiskem \"B\"","200ks",4.5277248924665336,{"$f":"F3666*(1-Elteq!$F$9)","v":4.5277248924665336},""]
["TECHNIK","PF 10/15",null,"Arch s etiketami bílá / žlutá, rozměr 15,0x4,7mm / 792 etiket na A4","10ks",54.926498695495653,{"$f":"F3667*(1-Elteq!$F$9)","v":54.926498695495653},"8591735013943"]
["TECHNIK","PF 10/21",null,"Arch s etiketami bílá / žlutá, rozměr 21,0x4,7mm / 594 etiket na A4","10ks",54.926498695495653,{"$f":"F3668*(1-Elteq!$F$9)","v":54.926498695495653},"8591735013936"]
["TECHNIK","PF 20/18",null,"Arch s etiketami bílá / žlutá, rozměr 17,5x9,5mm / 352 etiket na A4","10ks",72.369373281227382,{"$f":"F3669*(1-Elteq!$F$9)","v":72.369373281227382},""]
["TECHNIK","PM 10/33",null,"Průhledná pouzdra s kapsou 4,5x33mm","100ks",9.9461497637789424,{"$f":"F3670*(1-Elteq!$F$9)","v":9.9461497637789424},""]
["TECHNIK","PM 20/33",null,"Průhledná pouzdra s kapsou 9,5x33mm","100ks",12.61824970031657,{"$f":"F3671*(1-Elteq!$F$9)","v":12.61824970031657},""]
["TECHNIK","PM 20/45",null,"Průhledná pouzdra s kapsou 9,5x45mm","50ks",8.9069997884587551,{"$f":"F3672*(1-Elteq!$F$9)","v":8.9069997884587551},""]
["TECHNIK","PM 20/66",null,"Průhledná pouzdra s kapsou 9,5x66mm","50ks",12.61824970031657,{"$f":"F3673*(1-Elteq!$F$9)","v":12.61824970031657},""]
["TECHNIK","PM 24/33",null,"Průhledná pouzdra s kapsou 12x33mm","100ks",13.880074670348227,{"$f":"F3674*(1-Elteq!$F$9)","v":13.880074670348227},""]
["TECHNIK","PM 24/66",null,"Průhledná pouzdra s kapsou 12x66mm","50ks",13.880074670348227,{"$f":"F3675*(1-Elteq!$F$9)","v":13.880074670348227},""]
["TECHNIK","PTM 20",null,"Průhledné připínací kapsy, rozměr 4,6x23mm, pro uchycení jednou páskou","100ks",13.360499682688133,{"$f":"F3676*(1-Elteq!$F$9)","v":13.360499682688133},""]
["TECHNIK","PTM 30",null,"Průhledné připínací kapsy, rozměr 4,6x30mm, pro uchycení jednou páskou","500ks",64.946873457511757,{"$f":"F3677*(1-Elteq!$F$9)","v":64.946873457511757},"8591735029944"]
["TECHNIK","PTM 40",null,"Průhledné připínací kapsy, rozměr 4,6x39mm, pro uchycení dvěma páskami","100ks",12.98937469150235,{"$f":"F3678*(1-Elteq!$F$9)","v":12.98937469150235},""]
["TECHNIK","PK 2/4.40",null,"Návlečka žlutá bez potisku, délka 4mm","100ks",2.3009749453518449,{"$f":"F3679*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"-\"",null,"Návlečka žlutá s potiskem \"-\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3680*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"/\"",null,"Návlečka žlutá s potiskem \"/\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3681*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"0\"",null,"Návlečka žlutá s potiskem \"0\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3682*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"1\"",null,"Návlečka žlutá s potiskem \"1\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3683*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"2\"",null,"Návlečka žlutá s potiskem \"2\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3684*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"3\"",null,"Návlečka žlutá s potiskem \"3\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3685*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"4\"",null,"Návlečka žlutá s potiskem \"4\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3686*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"5\"",null,"Návlečka žlutá s potiskem \"5\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3687*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"6\"",null,"Návlečka žlutá s potiskem \"6\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3688*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"7\"",null,"Návlečka žlutá s potiskem \"7\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3689*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"8\"",null,"Návlečka žlutá s potiskem \"8\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3690*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"9\"",null,"Návlečka žlutá s potiskem \"9\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3691*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"A\"",null,"Návlečka žlutá s potiskem \"A\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3692*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"B\"",null,"Návlečka žlutá s potiskem \"B\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3693*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"C\"",null,"Návlečka žlutá s potiskem \"C\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3694*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"D\"",null,"Návlečka žlutá s potiskem \"D\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3695*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"E\"",null,"Návlečka žlutá s potiskem \"E\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3696*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"F\"",null,"Návlečka žlutá s potiskem \"F\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3697*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"G\"",null,"Návlečka žlutá s potiskem \"G\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3698*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"H\"",null,"Návlečka žlutá s potiskem \"H\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3699*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"I\"",null,"Návlečka žlutá s potiskem \"I\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3700*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"J\"",null,"Návlečka žlutá s potiskem \"J\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3701*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"K\"",null,"Návlečka žlutá s potiskem \"K\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3702*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"L\"",null,"Návlečka žlutá s potiskem \"L\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3703*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"M\"",null,"Návlečka žlutá s potiskem \"M\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3704*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"N\"",null,"Návlečka žlutá s potiskem \"N\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3705*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"O\"",null,"Návlečka žlutá s potiskem \"O\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3706*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"P\"",null,"Návlečka žlutá s potiskem \"P\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3707*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"Q\"",null,"Návlečka žlutá s potiskem \"Q\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3708*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"R\"",null,"Návlečka žlutá s potiskem \"R\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3709*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"S\"",null,"Návlečka žlutá s potiskem \"S\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3710*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"T\"",null,"Návlečka žlutá s potiskem \"T\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3711*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"U\"",null,"Návlečka žlutá s potiskem \"U\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3712*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"V\"",null,"Návlečka žlutá s potiskem \"V\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3713*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"W\"",null,"Návlečka žlutá s potiskem \"W\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3714*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"X\"",null,"Návlečka žlutá s potiskem \"X\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3715*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"Y\"",null,"Návlečka žlutá s potiskem \"Y\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3716*(1-Elteq!$F$9)","v":2.3009749453518449},""]
["TECHNIK","PK 2/4.40 \"Z\"",null,"Návlečka žlutá s potiskem \"Z\", délka 4mm","100ks",2.3009749453518449,{"$f":"F3717*(1-Elteq!$F$9)","v":2.3009749453518449},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"PK 2/5 \"0\"",null,"Návlečka žlutá s potiskem \"0\", délka 5mm (cívka)","500ks",11.504874726759224,{"$f":"F3718*(1-Elteq!$F$9)","v":11.504874726759224},""]
["TECHNIK","PK 2/5 \"1\"",null,"Návlečka žlutá s potiskem \"1\", délka 5mm (cívka)","500ks",11.504874726759224,{"$f":"F3719*(1-Elteq!$F$9)","v":11.504874726759224},""]
["TECHNIK","PK 2/5 \"2\"",null,"Návlečka žlutá s potiskem \"2\", délka 5mm (cívka)","500ks",11.504874726759224,{"$f":"F3720*(1-Elteq!$F$9)","v":11.504874726759224},""]
["TECHNIK","PK 2/5 \"3\"",null,"Návlečka žlutá s potiskem \"3\", délka 5mm (cívka)","500ks",11.504874726759224,{"$f":"F3721*(1-Elteq!$F$9)","v":11.504874726759224},""]
["TECHNIK","PK 2/5 \"4\"",null,"Návlečka žlutá s potiskem \"4\", délka 5mm (cívka)","500ks",11.504874726759224,{"$f":"F3722*(1-Elteq!$F$9)","v":11.504874726759224},""]
["TECHNIK","PK 2/5 \"5\"",null,"Návlečka žlutá s potiskem \"5\", délka 5mm (cívka)","500ks",11.504874726759224,{"$f":"F3723*(1-Elteq!$F$9)","v":11.504874726759224},""]
["TECHNIK","PK 2/5 \"6\"",null,"Návlečka žlutá s potiskem \"6\", délka 5mm (cívka)","500ks",11.504874726759224,{"$f":"F3724*(1-Elteq!$F$9)","v":11.504874726759224},""]
["TECHNIK","PK 2/5 \"7\"",null,"Návlečka žlutá s potiskem \"7\", délka 5mm (cívka)","500ks",11.504874726759224,{"$f":"F3725*(1-Elteq!$F$9)","v":11.504874726759224},""]
["TECHNIK","PK 2/5 \"8\"",null,"Návlečka žlutá s potiskem \"8\", délka 5mm (cívka)","500ks",11.504874726759224,{"$f":"F3726*(1-Elteq!$F$9)","v":11.504874726759224},""]
["TECHNIK","PK 2/5 \"9\"",null,"Návlečka žlutá s potiskem \"9\", délka 5mm (cívka)","500ks",11.504874726759224,{"$f":"F3727*(1-Elteq!$F$9)","v":11.504874726759224},""]
["TECHNIK","PKH 65",null,"Nosný pásek pro návlečky PK2, délka 65mm","100ks",7.7565123157828326,{"$f":"F3728*(1-Elteq!$F$9)","v":7.7565123157828326},"8591735012458"]
["TECHNIK","PKH 70",null,"Nosný pásek pro návlečky PK2, délka 70mm","100ks",7.4596123228342073,{"$f":"F3729*(1-Elteq!$F$9)","v":7.4596123228342073},"7330417021200"]
["TECHNIK","PKH 70 POL",null,"Nosný pásek pro bezhalogenové návlečky PKZ2, délka 70mm","100ks",16.737737102478743,{"$f":"F3730*(1-Elteq!$F$9)","v":16.737737102478743},""]
["TECHNIK","PKH100",null,"Nosný pásek pro návlečky PK2, délka 100mm","100ks",19.187162044304902,{"$f":"F3731*(1-Elteq!$F$9)","v":19.187162044304902},"8591735002428"]
["TECHNIK","PKH110 POL",null,"Nosný pásek pro bezhalogenové návlečky PKZ2, délka 110mm","100ks",19.261387042542058,{"$f":"F3732*(1-Elteq!$F$9)","v":19.261387042542058},""]
["TECHNIK","PLD \"0\"",null,"Cívky 5mm x 2,4m s čísly \"0\" pro PLD komplet","10ks",25.570511892700342,{"$f":"F3733*(1-Elteq!$F$9)","v":25.570511892700342},""]
["TECHNIK","PLD \"0-9\"",null,"Cívky 5mm x 2,4m s čísly \"0-9\" pro PLD komplet","10ks",25.570511892700342,{"$f":"F3734*(1-Elteq!$F$9)","v":25.570511892700342},""]
["TECHNIK","PLD \"1\"",null,"Cívky 5mm x 2,4m s čísly \"1\" pro PLD komplet","10ks",25.570511892700342,{"$f":"F3735*(1-Elteq!$F$9)","v":25.570511892700342},""]
["TECHNIK","PLD \"2\"",null,"Cívky 5mm x 2,4m s čísly \"2\" pro PLD komplet","10ks",25.570511892700342,{"$f":"F3736*(1-Elteq!$F$9)","v":25.570511892700342},""]
["TECHNIK","PLD \"3\"",null,"Cívky 5mm x 2,4m s čísly \"3\" pro PLD komplet","10ks",25.570511892700342,{"$f":"F3737*(1-Elteq!$F$9)","v":25.570511892700342},""]
["TECHNIK","PLD \"4\"",null,"Cívky 5mm x 2,4m s čísly \"4\" pro PLD komplet","10ks",25.570511892700342,{"$f":"F3738*(1-Elteq!$F$9)","v":25.570511892700342},""]
["TECHNIK","PLD \"5\"",null,"Cívky 5mm x 2,4m s čísly \"5\" pro PLD komplet","10ks",25.570511892700342,{"$f":"F3739*(1-Elteq!$F$9)","v":25.570511892700342},""]
["TECHNIK","PLD \"6\"",null,"Cívky 5mm x 2,4m s čísly \"6\" pro PLD komplet","10ks",25.570511892700342,{"$f":"F3740*(1-Elteq!$F$9)","v":25.570511892700342},""]
["TECHNIK","PLD \"7\"",null,"Cívky 5mm x 2,4m s čísly \"7\" pro PLD komplet","10ks",25.570511892700342,{"$f":"F3741*(1-Elteq!$F$9)","v":25.570511892700342},""]
["TECHNIK","PLD \"8\"",null,"Cívky 5mm x 2,4m s čísly \"8\" pro PLD komplet","10ks",25.570511892700342,{"$f":"F3742*(1-Elteq!$F$9)","v":25.570511892700342},""]
["TECHNIK","PLD \"9\"",null,"Cívky 5mm x 2,4m s čísly \"9\" pro PLD komplet","10ks",25.570511892700342,{"$f":"F3743*(1-Elteq!$F$9)","v":25.570511892700342},""]
["TECHNIK","PLD \"L\"",null,"Cívky 5mm x 2,4m se znaky \"L\" pro PLD komplet","10ks",25.570511892700342,{"$f":"F3744*(1-Elteq!$F$9)","v":25.570511892700342},""]
["TECHNIK","PLD \"L1\"",null,"Cívky 5mm x 2,4m se znaky \"L1\" pro PLD komplet","10ks",25.570511892700342,{"$f":"F3745*(1-Elteq!$F$9)","v":25.570511892700342},""]
["TECHNIK","PLD \"S\"",null,"Cívky 5mm x 2,4m se znaky \"S\" pro PLD komplet","10ks",25.570511892700342,{"$f":"F3746*(1-Elteq!$F$9)","v":25.570511892700342},""]
["TECHNIK","PLD \"zem\"",null,"Cívky 5mm x 2,4m se znaky \"zem\" pro PLD komplet","10ks",25.570511892700342,{"$f":"F3747*(1-Elteq!$F$9)","v":25.570511892700342},""]
["TECHNIK","PLD color",null,"Sada samolepicích značení vodičů - různé barvy","1sada",21.265461994945277,{"$f":"F3748*(1-Elteq!$F$9)","v":21.265461994945277},"8591735050559"]
["TECHNIK","PLD elektro",null,"Sada samolepicích značení vodičů - znaky elektro (L1,L2,L3,T1,T2,T3,+,-,PE,N)","1sada",21.265461994945277,{"$f":"F3749*(1-Elteq!$F$9)","v":21.265461994945277},"8591735050542"]
["TECHNIK","PLD komplet",null,"Sada samolepicích značení vodičů - čísla 0-9","1sada",21.265461994945277,{"$f":"F3750*(1-Elteq!$F$9)","v":21.265461994945277},"8591735042387"]
["TECHNIK","PLD pouzdro",null,"Prázdné pouzdro bez cívek","1ks",18.148012068984713,{"$f":"F3751*(1-Elteq!$F$9)","v":18.148012068984713},"8591735042370"]
["TECHNIK","TS 0",null,"Samolepicí štítky pro značení vodičů 5x7,5/20mm","910ks",12.432687204723679,{"$f":"F3752*(1-Elteq!$F$9)","v":12.432687204723679},""]
["TECHNIK","TS 1",null,"Samolepicí štítky pro značení vodičů 5x15/20mm","420ks",7.979187310494301,{"$f":"F3753*(1-Elteq!$F$9)","v":7.979187310494301},""]
["TECHNIK","TS 12",null,"Samolepicí štítky pro značení vodičů 7,5x15/30mm","270ks",12.98937469150235,{"$f":"F3754*(1-Elteq!$F$9)","v":12.98937469150235},""]
["TECHNIK","TS 2",null,"Samolepicí štítky pro značení vodičů 10x20/40mm","150ks",7.6080623193085195,{"$f":"F3755*(1-Elteq!$F$9)","v":7.6080623193085195},""]
["TECHNIK","TS 22",null,"Samolepicí štítky pro značení vodičů 10x10/40mm","280ks",7.979187310494301,{"$f":"F3756*(1-Elteq!$F$9)","v":7.979187310494301},""]
["TECHNIK","TS 3",null,"Samolepicí štítky pro značení vodičů 15x20/60mm","100ks",7.6080623193085195,{"$f":"F3757*(1-Elteq!$F$9)","v":7.6080623193085195},"8591735051457"]
["TECHNIK","TS 5",null,"Samolepicí štítky pro značení vodičů 25x25/100mm","50ks",7.6080623193085195,{"$f":"F3758*(1-Elteq!$F$9)","v":7.6080623193085195},""]
["TECHNIK","TS 51",null,"Samolepicí štítky pro značení vodičů 35x50/110mm","20ks",7.979187310494301,{"$f":"F3759*(1-Elteq!$F$9)","v":7.979187310494301},""]
["TECHNIK","TS 6",null,"Samolepicí štítky pro značení vodičů 25x25/120mm","40ks",7.6080623193085195,{"$f":"F3760*(1-Elteq!$F$9)","v":7.6080623193085195},""]
["TECHNIK","TS 61",null,"Samolepicí štítky pro značení vodičů 35x50/140mm","20ks",7.979187310494301,{"$f":"F3761*(1-Elteq!$F$9)","v":7.979187310494301},""]
["TECHNIK","PT 02/15",null,"Průhledné návlečky s kapsou pro průměr 1,2-2,0mm / průřez 0,25-1,5mm2 / délka 15mm","200ks",6.1606748536839726,{"$f":"F3762*(1-Elteq!$F$9)","v":6.1606748536839726},"7330417018634"]
["TECHNIK","PT 02/21",null,"Průhledné návlečky s kapsou pro průměr 1,2-2,0mm / průřez 0,25-1,5mm2 / délka 21mm","200ks",8.1647498060871921,{"$f":"F3763*(1-Elteq!$F$9)","v":8.1647498060871921},""]
["TECHNIK","PT 10/15",null,"Průhledné návlečky s kapsou pro průměr 2,5-5,0mm / průřez 1,5-4mm2 / délka 15mm","200ks",6.1606748536839726,{"$f":"F3764*(1-Elteq!$F$9)","v":6.1606748536839726},"7330417018958"]
["TECHNIK","PT 10/21",null,"Průhledné návlečky s kapsou pro průměr 2,5-5,0mm / průřez 1,5-4mm2 / délka 21mm","200ks",8.1647498060871921,{"$f":"F3765*(1-Elteq!$F$9)","v":8.1647498060871921},"7330417018965"]
["TECHNIK","PT 20/15",null,"Průhledné návlečky s kapsou pro průměr 4,0-10mm / průřez 2,5-16mm2 / délka 15mm","100ks",4.0823749030435961,{"$f":"F3766*(1-Elteq!$F$9)","v":4.0823749030435961},""]
["TECHNIK","PT 20/21",null,"Průhledné návlečky s kapsou pro průměr 4,0-10mm / průřez 2,5-16mm2 / délka 21mm","100ks",5.4184248713124097,{"$f":"F3767*(1-Elteq!$F$9)","v":5.4184248713124097},""]
["TECHNIK","PT 30/15",null,"Průhledné návlečky s kapsou pro průměr 8,0-16mm / průřez 16-75mm2 / délka 15mm","50ks",3.5627999153835019,{"$f":"F3768*(1-Elteq!$F$9)","v":3.5627999153835019},""]
["TECHNIK","PT 30/21",null,"Průhledné návlečky s kapsou pro průměr 8,0-16mm / průřez 16-75mm2 / délka 21mm","50ks",4.7503998871780029,{"$f":"F3769*(1-Elteq!$F$9)","v":4.7503998871780029},""]
["TECHNIK","PT 30/30",null,"Průhledné návlečky s kapsou pro průměr 8,0-16mm / průřez 16-75mm2 / délka 30mm","200ks",24.123124427075794,{"$f":"F3770*(1-Elteq!$F$9)","v":24.123124427075794},""]
["TECHNIK","PT 40/15",null,"Průhledné návlečky s kapsou pro průměr 14-22mm / průřez 50-95mm2 / délka 15mm","50ks",4.6390623898222678,{"$f":"F3771*(1-Elteq!$F$9)","v":4.6390623898222678},""]
["TECHNIK","PT 40/21",null,"Průhledné návlečky s kapsou pro průměr 14-22mm / průřez 50-95mm2 / délka 21mm","50ks",5.7153248642610341,{"$f":"F3772*(1-Elteq!$F$9)","v":5.7153248642610341},""]
["TECHNIK","PT 40/30",null,"Průhledné návlečky s kapsou pro průměr 14-22mm / průřez 50-95mm2 / délka 30mm","50ks",7.9420748113757229,{"$f":"F3773*(1-Elteq!$F$9)","v":7.9420748113757229},""]
["TECHNIK","PTC 10/15",null,"Žluté návlečky s kapsou pro průřez 1,5-2,0mm2 / průměr 2,4-3,0mm / délka 15mm","200ks",6.7915873386998005,{"$f":"F3774*(1-Elteq!$F$9)","v":6.7915873386998005},""]
["TECHNIK","PTC 10/21",null,"Žluté návlečky s kapsou pro průřez 1,5-2,0mm2 / průměr 2,4-3,0mm / délka 21mm","200ks",9.1296747831702234,{"$f":"F3775*(1-Elteq!$F$9)","v":9.1296747831702234},""]
["TECHNIK","PTC 10/30",null,"Žluté návlečky s kapsou pro průřez 1,5-2,0mm2 / průměr 2,4-3,0mm / délka 30mm","200ks",12.915149693265194,{"$f":"F3776*(1-Elteq!$F$9)","v":12.915149693265194},""]
["TECHNIK","PTC 20/15",null,"Žluté návlečky s kapsou pro průřez 2,0-2,5mm2 / průměr 3,0-4,0mm / délka 15mm","200ks",6.7915873386998005,{"$f":"F3777*(1-Elteq!$F$9)","v":6.7915873386998005},""]
["TECHNIK","PTC 20/21",null,"Žluté návlečky s kapsou pro průřez 2,0-2,5mm2 / průměr 3,0-4,0mm / délka 21mm","200ks",9.1296747831702234,{"$f":"F3778*(1-Elteq!$F$9)","v":9.1296747831702234},""]
["TECHNIK","PTC 20/30",null,"Žluté návlečky s kapsou pro průřez 2,0-2,5mm2 / průměr 3,0-4,0mm / délka 30mm","200ks",12.915149693265194,{"$f":"F3779*(1-Elteq!$F$9)","v":12.915149693265194},""]
["TECHNIK","PTC 30/15",null,"Žluté návlečky s kapsou pro průřez 2,5-4,0mm2 / průměr 4,0-5,0mm / délka 15mm","200ks",7.3482748254784731,{"$f":"F3780*(1-Elteq!$F$9)","v":7.3482748254784731},"8591735057114"]
["TECHNIK","PTC 30/21",null,"Žluté návlečky s kapsou pro průřez 2,5-4,0mm2 / průměr 4,0-5,0mm / délka 21mm","200ks",9.8348122664232083,{"$f":"F3781*(1-Elteq!$F$9)","v":9.8348122664232083},"8591735017583"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"PTC 30/30",null,"Žluté návlečky s kapsou pro průřez 2,5-4,0mm2 / průměr 4,0-5,0mm / délka 30mm","200ks",14.176974663296852,{"$f":"F3782*(1-Elteq!$F$9)","v":14.176974663296852},""]
["TECHNIK","PTC 40/15",null,"Žluté návlečky s kapsou pro průřez 4,0-6,0mm2 / průměr 5,0-6,2mm / délka 15mm","100ks",4.4906123933479556,{"$f":"F3783*(1-Elteq!$F$9)","v":4.4906123933479556},"8591735057121"]
["TECHNIK","PTC 40/21",null,"Žluté návlečky s kapsou pro průřez 4,0-6,0mm2 / průměr 5,0-6,2mm / délka 21mm","100ks",5.9379998589725034,{"$f":"F3784*(1-Elteq!$F$9)","v":5.9379998589725034},"8591735057138"]
["TECHNIK","PTC 40/30",null,"Žluté návlečky s kapsou pro průřez 4,0-6,0mm2 / průměr 5,0-6,2mm / délka 30mm","100ks",8.7585497919844428,{"$f":"F3785*(1-Elteq!$F$9)","v":8.7585497919844428},""]
["TECHNIK","PTC 50/15",null,"Žluté návlečky s kapsou pro průřez 5,0-7,0mm2 / průměr 6,0-7,2mm / délka 15mm","100ks",5.5668748677867219,{"$f":"F3786*(1-Elteq!$F$9)","v":5.5668748677867219},"8591735057145"]
["TECHNIK","PTC 50/21",null,"Žluté návlečky s kapsou pro průřez 5,0-7,0mm2 / průměr 6,0-7,2mm / délka 21mm","100ks",7.3482748254784731,{"$f":"F3787*(1-Elteq!$F$9)","v":7.3482748254784731},"8591735057152"]
["TECHNIK","PTC 50/30",null,"Žluté návlečky s kapsou pro průřez 5,0-7,0mm2 / průměr 6,0-7,2mm / délka 30mm","100ks",10.205937257608991,{"$f":"F3788*(1-Elteq!$F$9)","v":10.205937257608991},"8591735057169"]
["TECHNIK","AKR 1 - 60/24",null,"Smršťovací rozdělovací hlavice do 36 kV","1ks",28.725074317779484,{"$f":"F3789*(1-Elteq!$F$9)","v":28.725074317779484},""]
["TECHNIK","AKR 2 - 75/30",null,"Smršťovací rozdělovací hlavice do 36 kV","1ks",31.211611758724221,{"$f":"F3790*(1-Elteq!$F$9)","v":31.211611758724221},""]
["TECHNIK","AKR 3 - 110/45",null,"Smršťovací rozdělovací hlavice do 36 kV","1ks",33.58681170231322,{"$f":"F3791*(1-Elteq!$F$9)","v":33.58681170231322},""]
["TECHNIK","AKR 4 - 135/55",null,"Smršťovací rozdělovací hlavice do 36 kV","1ks",36.073349143257957,{"$f":"F3792*(1-Elteq!$F$9)","v":36.073349143257957},""]
["TECHNIK","AKR 5 - 175/55",null,"Smršťovací rozdělovací hlavice do 36 kV","1ks",38.596999083321272,{"$f":"F3793*(1-Elteq!$F$9)","v":38.596999083321272},""]
["TECHNIK","CCB 2 - 33/14",null,"Smršťovací rozdělovací hlavice pro průřez kabelu 1,5-25mm2 dvoužilová (SKR) 30/12","1ks",3.0803374268419863,{"$f":"F3794*(1-Elteq!$F$9)","v":3.0803374268419863},"8591735027360"]
["TECHNIK","CCB 2 - 50/21",null,"Smršťovací rozdělovací hlavice pro průřez kabelu 25-120mm2 dvoužilová (SKR)","1ks",8.4987622981543947,{"$f":"F3795*(1-Elteq!$F$9)","v":8.4987622981543947},"8591735027377"]
["TECHNIK","CCB 2 - 98/28",null,"Smršťovací rozdělovací hlavice pro průřez kabelu 120-240mm2 dvoužilová (SKR)","1ks",14.436762157126898,{"$f":"F3796*(1-Elteq!$F$9)","v":14.436762157126898},"8591735043759"]
["TECHNIK","CCB 3 - 25/9",null,"Smršťovací rozdělovací hlavice pro průřez kabelu 1,5-16mm2 třížilová (SKR)","1ks",4.4163873951107995,{"$f":"F3797*(1-Elteq!$F$9)","v":4.4163873951107995},"8591735043711"]
["TECHNIK","CCB 3 - 38/11",null,"Smršťovací rozdělovací hlavice pro průřez kabelu 4,0-35mm2 třížilová (SKR) 37/14","1ks",4.4906123933479556,{"$f":"F3798*(1-Elteq!$F$9)","v":4.4906123933479556},"8591735027384"]
["TECHNIK","CCB 3 - 60/24",null,"Smršťovací rozdělovací hlavice pro průřez kabelu 25-120mm2 třížilová (SKR) 65/27","1ks",7.1255998307670039,{"$f":"F3799*(1-Elteq!$F$9)","v":7.1255998307670039},"8591735027391"]
["TECHNIK","CCB 3 - 80/36",null,"Smršťovací rozdělovací hlavice pro průřez kabelu 95-240mm2 třížilová (SKR)","1ks",9.4265747761188496,{"$f":"F3800*(1-Elteq!$F$9)","v":9.4265747761188496},"8591735043728"]
["TECHNIK","CCB 3 -100/48",null,"Smršťovací rozdělovací hlavice pro průřez kabelu 95-300mm2 třížilová (SKR)","1ks",11.579099724996382,{"$f":"F3801*(1-Elteq!$F$9)","v":11.579099724996382},"8591735027407"]
["TECHNIK","CCB 3 -125/55",null,"Smršťovací rozdělovací hlavice pro průřez kabelu 150-300mm2 třížilová (SKR) 75/35","1ks",13.360499682688133,{"$f":"F3802*(1-Elteq!$F$9)","v":13.360499682688133},"8591735043766"]
["TECHNIK","CCB 3 -140/70",null,"Smršťovací rozdělovací hlavice pro průřez kabelu 185-400mm2 třížilová (SKR)","1ks",15.513024631565665,{"$f":"F3803*(1-Elteq!$F$9)","v":15.513024631565665},"8591735043735"]
["TECHNIK","CCB 4 - 28/9",null,"Smršťovací rozdělovací hlavice pro průřez kabelu 1,5-10mm2 čtyřžilová (SKR)","1ks",2.9318874303676736,{"$f":"F3804*(1-Elteq!$F$9)","v":2.9318874303676736},"8591735043742"]
["TECHNIK","CCB 4 - 38/11",null,"Smršťovací rozdělovací hlavice pro průřez kabelu 6,0-35mm2 čtyřžilová (SKR) 35/12","1ks",3.265899922434877,{"$f":"F3805*(1-Elteq!$F$9)","v":3.265899922434877},"8591735027353"]
["TECHNIK","CCB 4 - 55/20",null,"Smršťovací rozdělovací hlavice pro průřez kabelu 25-95mm2 čtyřžilová (SKR)","1ks",5.4184248713124097,{"$f":"F3806*(1-Elteq!$F$9)","v":5.4184248713124097},"8591735027414"]
["TECHNIK","CCB 4 - 75/25",null,"Smršťovací rozdělovací hlavice pro průřez kabelu 35-150mm2 čtyřžilová (SKR) 70/26","1ks",7.236937328122738,{"$f":"F3807*(1-Elteq!$F$9)","v":7.236937328122738},"8591735025403"]
["TECHNIK","CCB 4 -100/35",null,"Smršťovací rozdělovací hlavice pro průřez kabelu 95-300mm2 čtyřžilová (SKR) 90/35","1ks",11.02241223821771,{"$f":"F3808*(1-Elteq!$F$9)","v":11.02241223821771},"8591735021238"]
["TECHNIK","CCB 4 -125/45",null,"Smršťovací rozdělovací hlavice pro průřez kabelu 120-400mm2 čtyřžilová (SKR) 135/51","1ks",14.510987155364054,{"$f":"F3809*(1-Elteq!$F$9)","v":14.510987155364054},"8591735021245"]
["TECHNIK","CCB 5 - 38/12",null,"Smršťovací rozdělovací hlavice pro průřez kabelu 10-16mm2 pětižilová (SKR) 42/12","1ks",11.579099724996382,{"$f":"F3810*(1-Elteq!$F$9)","v":11.579099724996382},"8591735027438"]
["TECHNIK","CCB 5 - 53/15",null,"Smršťovací rozdělovací hlavice pro průřez kabelu 25-50mm2 pětižilová (SKR) 55/17","1ks",15.179012139498461,{"$f":"F3811*(1-Elteq!$F$9)","v":15.179012139498461},"8591735027421"]
["TECHNIK","CCB 5 - 80/26",null,"Smršťovací rozdělovací hlavice pro průřez kabelu 70-120mm2 pětižilová (SKR)","1ks",16.849074599834477,{"$f":"F3812*(1-Elteq!$F$9)","v":16.849074599834477},"8591735043780"]
["TECHNIK","CCB 5 -102/34",null,"Smršťovací rozdělovací hlavice pro průřez kabelu 150-240mm2 pětižilová (SKR)","1ks",17.888224575154666,{"$f":"F3813*(1-Elteq!$F$9)","v":17.888224575154666},"8591735043773"]
["TECHNIK","KT  40/15",null,"Smršťovací ochranná koncovka bez lepidla 40/15mm","1ks",1.3174937187095241,{"$f":"F3814*(1-Elteq!$F$9)","v":1.3174937187095241},"8591735040154"]
["TECHNIK","KTK  10/4",null,"Smršťovací ochranná koncovka s lepidlem 10/4mm (CEC,SKK)","1ks",0.68658123369369572,{"$f":"F3815*(1-Elteq!$F$9)","v":0.68658123369369572},"8591735018696"]
["TECHNIK","KTK  14/4",null,"Smršťovací ochranná koncovka s lepidlem 14/4mm (CEC,SKK)","1ks",0.70513748325298475,{"$f":"F3816*(1-Elteq!$F$9)","v":0.70513748325298475},"8591735051556"]
["TECHNIK","KTK  16/8",null,"Smršťovací ochranná koncovka s lepidlem 16/8mm (CEC,SKK)","1ks",0.98348122664232085,{"$f":"F3817*(1-Elteq!$F$9)","v":0.98348122664232085},"8591735051570"]
["TECHNIK","KTK  23/8",null,"Smršťovací ochranná koncovka s lepidlem 23/8mm (CEC,SKK)","1ks",1.020593725760899,{"$f":"F3818*(1-Elteq!$F$9)","v":1.020593725760899},"8591735018702"]
["TECHNIK","KTK  33/15",null,"Smršťovací ochranná koncovka s lepidlem 33/15mm (CEC,SKK)","1ks",1.1875999717945007,{"$f":"F3819*(1-Elteq!$F$9)","v":1.1875999717945007},"8591735018719"]
["TECHNIK","KTK  40/15",null,"Smršťovací ochranná koncovka s lepidlem 40/15mm (CEC,SKK)","1ks",1.3174937187095241,{"$f":"F3820*(1-Elteq!$F$9)","v":1.3174937187095241},"8591735027292"]
["TECHNIK","KTK  52/25",null,"Smršťovací ochranná koncovka s lepidlem 52/25mm (CEC,SKK)","1ks",2.3009749453518449,{"$f":"F3821*(1-Elteq!$F$9)","v":2.3009749453518449},"8591735027308"]
["TECHNIK","KTK  70/25",null,"Smršťovací ochranná koncovka s lepidlem 70/25mm (CEC,SKK)","1ks",2.5978749383004702,{"$f":"F3822*(1-Elteq!$F$9)","v":2.5978749383004702},"8591735027315"]
["TECHNIK","KTK  90/45",null,"Smršťovací ochranná koncovka s lepidlem 90/45mm (CEC,SKK)","1ks",3.7483624109763927,{"$f":"F3823*(1-Elteq!$F$9)","v":3.7483624109763927},"8591735027322"]
["TECHNIK","KTK 120/45",null,"Smršťovací ochranná koncovka s lepidlem 120/45mm (CEC,SKK)","1ks",4.7875123862965809,{"$f":"F3824*(1-Elteq!$F$9)","v":4.7875123862965809},"8591735027339"]
["TECHNIK","KTK 148/57",null,"Smršťovací ochranná koncovka s lepidlem 145/60mm (CEC,SKK)","1ks",7.9420748113757229,{"$f":"F3825*(1-Elteq!$F$9)","v":7.9420748113757229},"8591735027346"]
["TECHNIK","KTK 160/82",null,"Smršťovací ochranná koncovka s lepidlem 160/82mm (CEC,SKK)","1ks",10.948187239980554,{"$f":"F3826*(1-Elteq!$F$9)","v":10.948187239980554},"8591735047078"]
["TECHNIK","KTK 200/90",null,"Smršťovací ochranná koncovka s lepidlem 200/90mm (CEC,SKK)","1ks",12.98937469150235,{"$f":"F3827*(1-Elteq!$F$9)","v":12.98937469150235},"8591735051563"]
["TECHNIK","RM  22/6- 500",null,"Opravná smrštitelná manžeta s kovovým zipem rozměr 22/6mm, délka 500mm (SMO)","1ks",15.958374620988602,{"$f":"F3828*(1-Elteq!$F$9)","v":15.958374620988602},"8591735050825"]
["TECHNIK","RM  22/6-1000",null,"Opravná smrštitelná manžeta s kovovým zipem rozměr 22/6mm, délka 1000mm (SMO)","1ks",28.205499330119391,{"$f":"F3829*(1-Elteq!$F$9)","v":28.205499330119391},"8591735050818"]
["TECHNIK","RM  42/8- 500",null,"Opravná smrštitelná manžeta s kovovým zipem rozměr 42/8mm, délka 500mm (SMO)","1ks",17.62843708132462,{"$f":"F3830*(1-Elteq!$F$9)","v":17.62843708132462},"8591735018986"]
["TECHNIK","RM  42/8-1000",null,"Opravná smrštitelná manžeta s kovovým zipem rozměr 42/8mm, délka 1000mm (SMO)","1ks",31.545624250791423,{"$f":"F3831*(1-Elteq!$F$9)","v":31.545624250791423},"8591735019945"]
["TECHNIK","RM  42/8-1500",null,"Opravná smrštitelná manžeta s kovovým zipem rozměr 42/8mm, délka 1500mm (SMO)","1ks",47.132873880594246,{"$f":"F3832*(1-Elteq!$F$9)","v":47.132873880594246},"8591735027445"]
["TECHNIK","RM  62/22- 500",null,"Opravná smrštitelná manžeta s kovovým zipem rozměr 62/18mm, délka 500mm (SMO)","1ks",18.556249559289071,{"$f":"F3833*(1-Elteq!$F$9)","v":18.556249559289071},"8591735019969"]
["TECHNIK","RM  62/22-1000",null,"Opravná smrštitelná manžeta s kovovým zipem rozměr 62/18mm, délka 1000mm (SMO)","1ks",33.40124920672033,{"$f":"F3834*(1-Elteq!$F$9)","v":33.40124920672033},"8591735018993"]
["TECHNIK","RM  62/22-1500",null,"Opravná smrštitelná manžeta s kovovým zipem rozměr 62/18mm, délka 1500mm (SMO)","1ks",50.101873810080498,{"$f":"F3835*(1-Elteq!$F$9)","v":50.101873810080498},"8591735047030"]
["TECHNIK","RM  92/30- 500",null,"Opravná smrštitelná manžeta s kovovým zipem rozměr 92/25mm, délka 500mm (SMO)","1ks",21.154124497589542,{"$f":"F3836*(1-Elteq!$F$9)","v":21.154124497589542},"8591735019976"]
["TECHNIK","RM  92/30-1000",null,"Opravná smrštitelná manžeta s kovovým zipem rozměr 92/25mm, délka 1000mm (SMO)","1ks",38.596999083321272,{"$f":"F3837*(1-Elteq!$F$9)","v":38.596999083321272},"8591735019013"]
["TECHNIK","RM  92/30-1500",null,"Opravná smrštitelná manžeta s kovovým zipem rozměr 92/25mm, délka 1500mm (SMO)","1ks",58.081061120574802,{"$f":"F3838*(1-Elteq!$F$9)","v":58.081061120574802},"8591735019983"]
["TECHNIK","RM 122/38- 500",null,"Opravná smrštitelná manžeta s kovovým zipem rozměr 122/32mm, délka 500mm (SMO)","1ks",26.720999365376265,{"$f":"F3839*(1-Elteq!$F$9)","v":26.720999365376265},"8591735019990"]
["TECHNIK","RM 122/38-1000",null,"Opravná smrštitelná manžeta s kovovým zipem rozměr 122/32mm, délka 1000mm (SMO)","1ks",49.730748818894718,{"$f":"F3840*(1-Elteq!$F$9)","v":49.730748818894718},"8591735020002"]
["TECHNIK","RM 122/38-1500",null,"Opravná smrštitelná manžeta s kovovým zipem rozměr 122/32mm, délka 1500mm (SMO)","1ks",74.59612322834208,{"$f":"F3841*(1-Elteq!$F$9)","v":74.59612322834208},"8591735033804"]
["TECHNIK","RM 160/40- 500",null,"Opravná smrštitelná manžeta s kovovým zipem rozměr 160/40mm, délka 500mm (SMO)","1ks",32.102311737570098,{"$f":"F3842*(1-Elteq!$F$9)","v":32.102311737570098},"8591735050849"]
["TECHNIK","RM 160/40-1000",null,"Opravná smrštitelná manžeta s kovovým zipem rozměr 160/40mm, délka 1000mm (SMO)","1ks",60.493373563282375,{"$f":"F3843*(1-Elteq!$F$9)","v":60.493373563282375},"8591735050832"]
["TECHNIK","RM 210/55- 500",null,"Opravná smrštitelná manžeta s kovovým zipem rozměr 210/55mm, délka 500mm (SMO)","1ks",35.999124145020801,{"$f":"F3844*(1-Elteq!$F$9)","v":35.999124145020801},"8591735020019"]
["TECHNIK","RM 210/55-1000",null,"Opravná smrštitelná manžeta s kovovým zipem rozměr 210/55mm, délka 1000mm (SMO)","1ks",68.286998378183782,{"$f":"F3845*(1-Elteq!$F$9)","v":68.286998378183782},"8591735020026"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"RM 210/55-1500",null,"Opravná smrštitelná manžeta s kovovým zipem rozměr 210/55mm, délka 1500mm (SMO)","1ks",102.24493507168279,{"$f":"F3846*(1-Elteq!$F$9)","v":102.24493507168279},"8591735020033"]
["TECHNIK","TKT  25",null,"Smršťovací elektroizolační pás šíře 25mm, síla pásu 1,0mm / vrstva lepidla 0,1mm","15m",23.937561931482904,{"$f":"F3847*(1-Elteq!$F$9)","v":23.937561931482904},"8591735045425"]
["TECHNIK","TKT  50",null,"Smršťovací elektroizolační pás šíře 50mm, síla pásu 1,0mm / vrstva lepidla 0,1mm","15m",49.916311314487608,{"$f":"F3848*(1-Elteq!$F$9)","v":49.916311314487608},"8591735045432"]
["TECHNIK","TKT  75",null,"Smršťovací elektroizolační pás šíře 75mm, síla pásu 1,0mm / vrstva lepidla 0,1mm","15m",74.59612322834208,{"$f":"F3849*(1-Elteq!$F$9)","v":74.59612322834208},"8591735045500"]
["TECHNIK","TKT 100",null,"Smršťovací elektroizolační pás šíře 100mm, síla pásu 1,0mm / vrstva lepidla 0,1mm","15m",98.348122664232093,{"$f":"F3850*(1-Elteq!$F$9)","v":98.348122664232093},"8591735045449"]
["TECHNIK","TKT 150",null,"Smršťovací elektroizolační pás šíře 150mm, síla pásu 1,0mm / vrstva lepidla 0,1mm","15m",151.23343390820594,{"$f":"F3851*(1-Elteq!$F$9)","v":151.23343390820594},"8591735045418"]
["TECHNIK","Sada PBF",null,"Sada smršťovacích trubic PBF a s lepidlem RCK vč. stojanu","1sada",240.1178692972006,{"$f":"F3852*(1-Elteq!$F$9)","v":240.1178692972006},"8591735027452"]
["TECHNIK","SLV   2,5-10",null,"Smršťovací trubice čtyřžilová 4x2,5 až 4x10mm2","1sada",3.2287874233162985,{"$f":"F3853*(1-Elteq!$F$9)","v":3.2287874233162985},"8591735047955"]
["TECHNIK","SLV   6-25",null,"Smršťovací trubice čtyřžilová 4x6 až 4x25mm2","1sada",6.9400373351741136,{"$f":"F3854*(1-Elteq!$F$9)","v":6.9400373351741136},"8591735020101"]
["TECHNIK","SLV   6-25/5",null,"Smršťovací trubice pětižilová 5x6 až 5x25mm2","1sada",7.5709498201899414,{"$f":"F3855*(1-Elteq!$F$9)","v":7.5709498201899414},"8591735047993"]
["TECHNIK","SLV  16-70",null,"Smršťovací trubice čtyřžilová 4x16 až 4x70mm2","1sada",14.548099654482634,{"$f":"F3856*(1-Elteq!$F$9)","v":14.548099654482634},"8591735047962"]
["TECHNIK","SLV  35-185",null,"Smršťovací trubice čtyřžilová 4x35 až 4x185mm2","1sada",19.446949538134948,{"$f":"F3857*(1-Elteq!$F$9)","v":19.446949538134948},"8591735036935"]
["TECHNIK","SLV 120-240",null,"Smršťovací trubice čtyřžilová 4x120 až 4x240mm2","1sada",34.811524173226303,{"$f":"F3858*(1-Elteq!$F$9)","v":34.811524173226303},"8591735047979"]
["TECHNIK","SLV 240/1x120",null,"Smršťovací trubice čtyřžilová 3x240 + 1x120mm2","1sada",24.38291192090584,{"$f":"F3859*(1-Elteq!$F$9)","v":24.38291192090584},"8591735047986"]
["TECHNIK","Stojan PBF",null,"Stojan pro smršťovací trubice PBF a RCK (prázdný bez trubic)","1sada",139.17187169466806,{"$f":"F3860*(1-Elteq!$F$9)","v":139.17187169466806},"8591735050566"]
["TECHNIK","UNISET black",null,"Sada smršťovacích trubic HTI v plastovém boxu - černé, samozhášivé","1sada",11.096637236454866,{"$f":"F3861*(1-Elteq!$F$9)","v":11.096637236454866},"8591735048419"]
["TECHNIK","UNISET color",null,"Sada smršťovacích trubic HTI v plastovém boxu - barevné, samozhášivé","1sada",11.096637236454866,{"$f":"F3862*(1-Elteq!$F$9)","v":11.096637236454866},"8591735037307"]
["TECHNIK","UNISET PBF",null,"Sada smršťovacích trubic PBF v plastovém boxu - barevné, lesklé","1sada",11.690437222352116,{"$f":"F3863*(1-Elteq!$F$9)","v":11.690437222352116},"8591735016531"]
["TECHNIK","ZID4-M",null,"Smršťovací trubice čtyřžilová 4x2,5 až 4x6mm2 / 4 žíly v černé barvě","1sada",1.8927374550474854,{"$f":"F3864*(1-Elteq!$F$9)","v":1.8927374550474854},"8591735013950"]
["TECHNIK","ZID4-M žz",null,"Smršťovací trubice čtyřžilová 4x2,5 až 4x6mm2 / 1 žíla žluto-zelená","1sada",2.3009749453518449,{"$f":"F3865*(1-Elteq!$F$9)","v":2.3009749453518449},"8591735018191"]
["TECHNIK","ZID4-M0",null,"Smršťovací trubice čtyřžilová 4x6 až 4x16mm2 / 4 žíly v černé barvě","1sada",4.2308248995179083,{"$f":"F3866*(1-Elteq!$F$9)","v":4.2308248995179083},"8591735013011"]
["TECHNIK","ZID4-M0 žz",null,"Smršťovací trubice čtyřžilová 4x6 až 4x16mm2 / 1 žíla žluto-zelená","1sada",4.6390623898222678,{"$f":"F3867*(1-Elteq!$F$9)","v":4.6390623898222678},"8591735017040"]
["TECHNIK","ZID4-M1",null,"Smršťovací trubice čtyřžilová 4x16 až 4x35mm2 / 4 žíly v černé barvě","1sada",6.5689123439883321,{"$f":"F3868*(1-Elteq!$F$9)","v":6.5689123439883321},"8591735013004"]
["TECHNIK","ZID4-M1 žz",null,"Smršťovací trubice čtyřžilová 4x16 až 4x35mm2 / 1 žíla žluto-zelená","1sada",7.1255998307670039,{"$f":"F3869*(1-Elteq!$F$9)","v":7.1255998307670039},"8591735017057"]
["TECHNIK","ZID4-M2",null,"Smršťovací trubice čtyřžilová 4x50 až 4x120mm2 / 4 žíly v černé barvě","1sada",10.391499753201881,{"$f":"F3870*(1-Elteq!$F$9)","v":10.391499753201881},"8591735012991"]
["TECHNIK","ZID4-M2 žz",null,"Smršťovací trubice čtyřžilová 4x50 až 4x120mm2 / 1 žíla žluto-zelená","1sada",10.799737243506241,{"$f":"F3871*(1-Elteq!$F$9)","v":10.799737243506241},"8591735020132"]
["TECHNIK","ZID4-M3",null,"Smršťovací trubice čtyřžilová 4x150 až 4x240mm2 / 4 žíly v černé barvě","1sada",17.702662079561776,{"$f":"F3872*(1-Elteq!$F$9)","v":17.702662079561776},"8591735012984"]
["TECHNIK","ZID4-M3 žz",null,"Smršťovací trubice čtyřžilová 4x150 až 4x240mm2 / 1 žíla žluto-zelená","1sada",18.148012068984713,{"$f":"F3873*(1-Elteq!$F$9)","v":18.148012068984713},"8591735020149"]
["TECHNIK","ZID4-M4",null,"Smršťovací trubice čtyřžilová 4x120 až 4x240mm2 / 4 žíly v černé barvě (verze pro šroubové spojky)","1sada",28.947749312490952,{"$f":"F3874*(1-Elteq!$F$9)","v":28.947749312490952},"8591735055844"]
["TECHNIK","ZID4-M5",null,"Smršťovací trubice čtyřžilová 4x1,5 až 4x16mm2 / 4 žíly v černé barvě (verze pro šroubové spojky)","1sada",16.997524596308789,{"$f":"F3875*(1-Elteq!$F$9)","v":16.997524596308789},"8591735055837"]
["TECHNIK","ZID5-M",null,"Smršťovací trubice pětižilová 5x2,5 až 5x6mm2 / 5 žil v černé barvě","1sada",2.0782999506403761,{"$f":"F3876*(1-Elteq!$F$9)","v":2.0782999506403761},"8591735016432"]
["TECHNIK","ZID5-M žz",null,"Smršťovací trubice pětižilová 5x2,5 až 5x6mm2 / 1 žíla žluto-zelená","1sada",2.5236499400633141,{"$f":"F3877*(1-Elteq!$F$9)","v":2.5236499400633141},"8591735019068"]
["TECHNIK","ZID5-M0",null,"Smršťovací trubice pětižilová 5x6 až 5x16mm2 / 5 žil v černé barvě","1sada",4.7132873880594248,{"$f":"F3878*(1-Elteq!$F$9)","v":4.7132873880594248},"8591735017019"]
["TECHNIK","ZID5-M0 žz",null,"Smršťovací trubice pětižilová 5x6 až 5x16mm2 / 1 žíla žluto-zelená","1sada",5.1586373774823624,{"$f":"F3879*(1-Elteq!$F$9)","v":5.1586373774823624},"8591735017156"]
["TECHNIK","ZID5-M1",null,"Smršťovací trubice pětižilová 5x16 až 5x35mm2 / 5 žil v černé barvě","1sada",7.1255998307670039,{"$f":"F3880*(1-Elteq!$F$9)","v":7.1255998307670039},"8591735017026"]
["TECHNIK","ZID5-M1 žz",null,"Smršťovací trubice pětižilová 5x16 až 5x35mm2 / 1 žíla žluto-zelená","1sada",7.6822873175456765,{"$f":"F3881*(1-Elteq!$F$9)","v":7.6822873175456765},"8591735017163"]
["TECHNIK","ZID5-M2",null,"Smršťovací trubice pětižilová 5x50 až 5x120mm2 / 5 žil v černé barvě","1sada",11.170862234692022,{"$f":"F3882*(1-Elteq!$F$9)","v":11.170862234692022},"8591735017033"]
["TECHNIK","ZID5-M2 žz",null,"Smršťovací trubice pětižilová 5x50 až 5x120mm2 / 1 žíla žluto-zelená","1sada",11.690437222352116,{"$f":"F3883*(1-Elteq!$F$9)","v":11.690437222352116},"8591735017170"]
["TECHNIK","ZID5-M3 žz",null,"Smršťovací trubice pětižilová 5x150 až 5x240mm2 / 1 žíla žluto-zelená","1sada",17.108862093664523,{"$f":"F3884*(1-Elteq!$F$9)","v":17.108862093664523},"8591735030018"]
["TECHNIK","RDK  76/18",null,"Smršťovací trubice extra velká s lepidlem, rozměr 76,0/18,0mm černá","1m",15.884149622751446,{"$f":"F3885*(1-Elteq!$F$9)","v":15.884149622751446},""]
["TECHNIK","RDK 105/32",null,"Smršťovací trubice extra velká s lepidlem, rozměr 105,0/32,0mm černá","1m",19.59539953460926,{"$f":"F3886*(1-Elteq!$F$9)","v":19.59539953460926},""]
["TECHNIK","RDK 140/34",null,"Smršťovací trubice extra velká s lepidlem, rozměr 140,0/34,0mm černá","1m",23.046861952637027,{"$f":"F3887*(1-Elteq!$F$9)","v":23.046861952637027},""]
["TECHNIK","RDK 155/90",null,"Smršťovací trubice extra velká s lepidlem, rozměr 155,0/90,0mm černá","1m",29.912674289573985,{"$f":"F3888*(1-Elteq!$F$9)","v":29.912674289573985},""]
["TECHNIK","RDK 175/77",null,"Smršťovací trubice extra velká s lepidlem, rozměr 175,0/77,0mm černá","1m",38.968124074507053,{"$f":"F3889*(1-Elteq!$F$9)","v":38.968124074507053},""]
["TECHNIK","RDK 185/42",null,"Smršťovací trubice extra velká s lepidlem, rozměr 185,0/42,0mm černá","1m",40.081499048064394,{"$f":"F3890*(1-Elteq!$F$9)","v":40.081499048064394},""]
["TECHNIK","RDK 225/90",null,"Smršťovací trubice extra velká s lepidlem, rozměr 225,0/90,0mm černá","1m",29.912674289573985,{"$f":"F3891*(1-Elteq!$F$9)","v":29.912674289573985},""]
["TECHNIK","RDK 245/125",null,"Smršťovací trubice extra velká s lepidlem, rozměr 245,0/125,0mm černá","1m",67.730310891405111,{"$f":"F3892*(1-Elteq!$F$9)","v":67.730310891405111},""]
["TECHNIK","RDK 350/125",null,"Smršťovací trubice extra velká s lepidlem, rozměr 350,0/125,0mm černá","1m",67.730310891405111,{"$f":"F3893*(1-Elteq!$F$9)","v":67.730310891405111},""]
["TECHNIK","RDK 390/200",null,"Smršťovací trubice extra velká s lepidlem, rozměr 390,0/200,0mm černá","1m",95.898697722405927,{"$f":"F3894*(1-Elteq!$F$9)","v":95.898697722405927},"8591735042691"]
["TECHNIK","RDK 500/200",null,"Smršťovací trubice extra velká s lepidlem, rozměr 500,0/200,0mm černá","1m",95.898697722405927,{"$f":"F3895*(1-Elteq!$F$9)","v":95.898697722405927},""]
["TECHNIK","RDK 710/250",null,"Smršťovací trubice extra velká s lepidlem, rozměr 710,0/250,0mm černá","1m",120.61562213537897,{"$f":"F3896*(1-Elteq!$F$9)","v":120.61562213537897},""]
["TECHNIK","RDK 820/315",null,"Smršťovací trubice extra velká s lepidlem, rozměr 820,0/315,0mm černá","1m",129.70818441943061,{"$f":"F3897*(1-Elteq!$F$9)","v":129.70818441943061},""]
["TECHNIK","RDK 920/315",null,"Smršťovací trubice extra velká s lepidlem, rozměr 920,0/315,0mm černá","1m",131.74937187095242,{"$f":"F3898*(1-Elteq!$F$9)","v":131.74937187095242},""]
["TECHNIK","HTN  1,2/20 bílá",null,"Nasekaná smršťovací trubice 1,2/0,6mm bílá / 20mm","1000ks",11.579099724996382,{"$f":"F3899*(1-Elteq!$F$9)","v":11.579099724996382},""]
["TECHNIK","HTN  1,2/20 černá",null,"Nasekaná smršťovací trubice 1,2/0,6mm černá / 20mm","1000ks",11.579099724996382,{"$f":"F3900*(1-Elteq!$F$9)","v":11.579099724996382},""]
["TECHNIK","HTN  1,2/20 modrá",null,"Nasekaná smršťovací trubice 1,2/0,6mm modrá / 20mm","1000ks",11.579099724996382,{"$f":"F3901*(1-Elteq!$F$9)","v":11.579099724996382},""]
["TECHNIK","HTN  1,2/20 rudá",null,"Nasekaná smršťovací trubice 1,2/0,6mm rudá / 20mm","1000ks",11.579099724996382,{"$f":"F3902*(1-Elteq!$F$9)","v":11.579099724996382},""]
["TECHNIK","HTN  1,2/20 zelená",null,"Nasekaná smršťovací trubice 1,2/0,6mm zelená/ 20mm","1000ks",11.579099724996382,{"$f":"F3903*(1-Elteq!$F$9)","v":11.579099724996382},""]
["TECHNIK","HTN  1,2/20 žlutá",null,"Nasekaná smršťovací trubice 1,2/0,6mm žlutá / 20mm","1000ks",11.579099724996382,{"$f":"F3904*(1-Elteq!$F$9)","v":11.579099724996382},""]
["TECHNIK","HTN  1,2/30 černá",null,"Nasekaná smršťovací trubice 1,2/0,6mm černá / 30mm","1000ks",14.696549650956946,{"$f":"F3905*(1-Elteq!$F$9)","v":14.696549650956946},"8591735045906"]
["TECHNIK","HTN  1,2/30 transp",null,"Nasekaná smršťovací trubice 1,2/0,6mm transparentní / 30mm","1000ks",14.696549650956946,{"$f":"F3906*(1-Elteq!$F$9)","v":14.696549650956946},""]
["TECHNIK","HTN  1,6/20 bílá",null,"Nasekaná smršťovací trubice 1,6/0,8mm bílá / 20mm","1000ks",11.579099724996382,{"$f":"F3907*(1-Elteq!$F$9)","v":11.579099724996382},""]
["TECHNIK","HTN  1,6/20 černá",null,"Nasekaná smršťovací trubice 1,6/0,8mm černá / 20mm","1000ks",11.579099724996382,{"$f":"F3908*(1-Elteq!$F$9)","v":11.579099724996382},""]
["TECHNIK","HTN  1,6/20 modrá",null,"Nasekaná smršťovací trubice 1,6/0,8mm modrá / 20mm","1000ks",11.579099724996382,{"$f":"F3909*(1-Elteq!$F$9)","v":11.579099724996382},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"HTN  1,6/20 rudá",null,"Nasekaná smršťovací trubice 1,6/0,8mm rudá / 20mm","1000ks",11.579099724996382,{"$f":"F3910*(1-Elteq!$F$9)","v":11.579099724996382},""]
["TECHNIK","HTN  1,6/20 zelená",null,"Nasekaná smršťovací trubice 1,6/0,8mm zelená/ 20mm","1000ks",11.579099724996382,{"$f":"F3911*(1-Elteq!$F$9)","v":11.579099724996382},""]
["TECHNIK","HTN  1,6/20 žlutá",null,"Nasekaná smršťovací trubice 1,6/0,8mm žlutá / 20mm","1000ks",11.579099724996382,{"$f":"F3912*(1-Elteq!$F$9)","v":11.579099724996382},""]
["TECHNIK","HTN  1,6/25 transp",null,"Nasekaná smršťovací trubice 1,6/0,8mm transparentní / 25mm","1000ks",14.696549650956946,{"$f":"F3913*(1-Elteq!$F$9)","v":14.696549650956946},""]
["TECHNIK","HTN  1,6/30 bílá",null,"Nasekaná smršťovací trubice 1,6/0,8mm bílá / 30mm","1000ks",14.696549650956946,{"$f":"F3914*(1-Elteq!$F$9)","v":14.696549650956946},""]
["TECHNIK","HTN  1,6/30 černá",null,"Nasekaná smršťovací trubice 1,6/0,8mm černá / 30mm","1000ks",14.696549650956946,{"$f":"F3915*(1-Elteq!$F$9)","v":14.696549650956946},"8591735045913"]
["TECHNIK","HTN  1,6/30 modrá",null,"Nasekaná smršťovací trubice 1,6/0,8mm modrá / 30mm","1000ks",14.696549650956946,{"$f":"F3916*(1-Elteq!$F$9)","v":14.696549650956946},""]
["TECHNIK","HTN  1,6/30 rudá",null,"Nasekaná smršťovací trubice 1,6/0,8mm rudá / 30mm","1000ks",14.696549650956946,{"$f":"F3917*(1-Elteq!$F$9)","v":14.696549650956946},""]
["TECHNIK","HTN  1,6/30 šedá",null,"Nasekaná smršťovací trubice 1,6/0,8mm šedá / 30mm","1000ks",14.696549650956946,{"$f":"F3918*(1-Elteq!$F$9)","v":14.696549650956946},""]
["TECHNIK","HTN  2,4/15 černá",null,"Nasekaná smršťovací trubice 2,4/1,2mm černá / 15mm","1000ks",12.469799703842257,{"$f":"F3919*(1-Elteq!$F$9)","v":12.469799703842257},"8591735043001"]
["TECHNIK","HTN  2,4/20 bílá",null,"Nasekaná smršťovací trubice 2,4/1,2mm bílá / 20mm","1000ks",12.469799703842257,{"$f":"F3920*(1-Elteq!$F$9)","v":12.469799703842257},""]
["TECHNIK","HTN  2,4/20 černá",null,"Nasekaná smršťovací trubice 2,4/1,2mm černá / 20mm","1000ks",12.469799703842257,{"$f":"F3921*(1-Elteq!$F$9)","v":12.469799703842257},""]
["TECHNIK","HTN  2,4/20 modrá",null,"Nasekaná smršťovací trubice 2,4/1,2mm modrá / 20mm","1000ks",12.469799703842257,{"$f":"F3922*(1-Elteq!$F$9)","v":12.469799703842257},""]
["TECHNIK","HTN  2,4/20 rudá",null,"Nasekaná smršťovací trubice 2,4/1,2mm rudá / 20mm","1000ks",12.469799703842257,{"$f":"F3923*(1-Elteq!$F$9)","v":12.469799703842257},""]
["TECHNIK","HTN  2,4/20 zelená",null,"Nasekaná smršťovací trubice 2,4/1,2mm zelená / 20mm","1000ks",12.469799703842257,{"$f":"F3924*(1-Elteq!$F$9)","v":12.469799703842257},""]
["TECHNIK","HTN  2,4/20 žlutá",null,"Nasekaná smršťovací trubice 2,4/1,2mm žlutá / 20mm","1000ks",12.469799703842257,{"$f":"F3925*(1-Elteq!$F$9)","v":12.469799703842257},""]
["TECHNIK","HTN  2,4/30 bílá",null,"Nasekaná smršťovací trubice 2,4/1,2mm bílá / 30mm","1000ks",16.03259961922576,{"$f":"F3926*(1-Elteq!$F$9)","v":16.03259961922576},""]
["TECHNIK","HTN  2,4/30 černá",null,"Nasekaná smršťovací trubice 2,4/1,2mm černá / 30mm","1000ks",16.03259961922576,{"$f":"F3927*(1-Elteq!$F$9)","v":16.03259961922576},"8591735045920"]
["TECHNIK","HTN  2,4/30 hnědá",null,"Nasekaná smršťovací trubice 2,4/1,2mm hnědá / 30mm","1000ks",16.03259961922576,{"$f":"F3928*(1-Elteq!$F$9)","v":16.03259961922576},""]
["TECHNIK","HTN  2,4/30 modrá",null,"Nasekaná smršťovací trubice 2,4/1,2mm modrá / 30mm","1000ks",16.03259961922576,{"$f":"F3929*(1-Elteq!$F$9)","v":16.03259961922576},""]
["TECHNIK","HTN  2,4/30 rudá",null,"Nasekaná smršťovací trubice 2,4/1,2mm rudá / 30mm","1000ks",16.03259961922576,{"$f":"F3930*(1-Elteq!$F$9)","v":16.03259961922576},""]
["TECHNIK","HTN  2,4/30 šedá",null,"Nasekaná smršťovací trubice 2,4/1,2mm šedá / 30mm","1000ks",16.03259961922576,{"$f":"F3931*(1-Elteq!$F$9)","v":16.03259961922576},""]
["TECHNIK","HTN  2,4/30 transp",null,"Nasekaná smršťovací trubice 2,4/1,2mm transparentní / 30mm","1000ks",16.03259961922576,{"$f":"F3932*(1-Elteq!$F$9)","v":16.03259961922576},""]
["TECHNIK","HTN  2,4/30 žz",null,"Nasekaná smršťovací trubice 2,4/1,2mm žluto-zelená / 30mm","1000ks",20.931449502878074,{"$f":"F3933*(1-Elteq!$F$9)","v":20.931449502878074},""]
["TECHNIK","HTN  3,2/20 bílá",null,"Nasekaná smršťovací trubice 3,2/1,6mm bílá / 20mm","1000ks",12.469799703842257,{"$f":"F3934*(1-Elteq!$F$9)","v":12.469799703842257},""]
["TECHNIK","HTN  3,2/20 černá",null,"Nasekaná smršťovací trubice 3,2/1,6mm černá / 20mm","1000ks",12.469799703842257,{"$f":"F3935*(1-Elteq!$F$9)","v":12.469799703842257},""]
["TECHNIK","HTN  3,2/20 modrá",null,"Nasekaná smršťovací trubice 3,2/1,6mm modrá / 20mm","1000ks",12.469799703842257,{"$f":"F3936*(1-Elteq!$F$9)","v":12.469799703842257},""]
["TECHNIK","HTN  3,2/20 rudá",null,"Nasekaná smršťovací trubice 3,2/1,6mm rudá / 20mm","1000ks",12.469799703842257,{"$f":"F3937*(1-Elteq!$F$9)","v":12.469799703842257},""]
["TECHNIK","HTN  3,2/20 transp",null,"Nasekaná smršťovací trubice 3,2/1,6mm transparentní / 20mm","1000ks",12.469799703842257,{"$f":"F3938*(1-Elteq!$F$9)","v":12.469799703842257},""]
["TECHNIK","HTN  3,2/20 zelená",null,"Nasekaná smršťovací trubice 3,2/1,6mm zelená / 20mm","1000ks",12.469799703842257,{"$f":"F3939*(1-Elteq!$F$9)","v":12.469799703842257},""]
["TECHNIK","HTN  3,2/20 žlutá",null,"Nasekaná smršťovací trubice 3,2/1,6mm žlutá / 20mm","1000ks",12.469799703842257,{"$f":"F3940*(1-Elteq!$F$9)","v":12.469799703842257},""]
["TECHNIK","HTN  3,2/30 bílá",null,"Nasekaná smršťovací trubice 3,2/1,6mm bílá / 30mm","1000ks",16.03259961922576,{"$f":"F3941*(1-Elteq!$F$9)","v":16.03259961922576},""]
["TECHNIK","HTN  3,2/30 černá",null,"Nasekaná smršťovací trubice 3,2/1,6mm černá / 30mm","1000ks",16.03259961922576,{"$f":"F3942*(1-Elteq!$F$9)","v":16.03259961922576},"8591735045937"]
["TECHNIK","HTN  3,2/30 modrá",null,"Nasekaná smršťovací trubice 3,2/1,6mm modrá / 30mm","1000ks",16.03259961922576,{"$f":"F3943*(1-Elteq!$F$9)","v":16.03259961922576},""]
["TECHNIK","HTN  3,2/30 rudá",null,"Nasekaná smršťovací trubice 3,2/1,6mm rudá / 30mm","1000ks",16.03259961922576,{"$f":"F3944*(1-Elteq!$F$9)","v":16.03259961922576},""]
["TECHNIK","HTN  3,2/30 šedá",null,"Nasekaná smršťovací trubice 3,2/1,6mm šedá / 30mm","1000ks",16.03259961922576,{"$f":"F3945*(1-Elteq!$F$9)","v":16.03259961922576},""]
["TECHNIK","HTN  3,2/30 transp",null,"Nasekaná smršťovací trubice 3,2/1,6mm transparentní / 30mm","1000ks",16.03259961922576,{"$f":"F3946*(1-Elteq!$F$9)","v":16.03259961922576},""]
["TECHNIK","HTN  3,2/30 žlutá",null,"Nasekaná smršťovací trubice 3,2/1,6mm žlutá / 30mm","1000ks",16.03259961922576,{"$f":"F3947*(1-Elteq!$F$9)","v":16.03259961922576},""]
["TECHNIK","HTN  3,2/30 žz",null,"Nasekaná smršťovací trubice 3,2/1,6mm žluto-zelená / 30mm","1000ks",22.267499471146888,{"$f":"F3948*(1-Elteq!$F$9)","v":22.267499471146888},""]
["TECHNIK","HTN  4,8/20 bílá",null,"Nasekaná smršťovací trubice 4,8/2,4mm bílá / 20mm","1000ks",14.696549650956946,{"$f":"F3949*(1-Elteq!$F$9)","v":14.696549650956946},""]
["TECHNIK","HTN  4,8/20 černá",null,"Nasekaná smršťovací trubice 4,8/2,4mm černá / 20mm","1000ks",14.696549650956946,{"$f":"F3950*(1-Elteq!$F$9)","v":14.696549650956946},""]
["TECHNIK","HTN  4,8/20 modrá",null,"Nasekaná smršťovací trubice 4,8/2,4mm modrá / 20mm","1000ks",14.696549650956946,{"$f":"F3951*(1-Elteq!$F$9)","v":14.696549650956946},""]
["TECHNIK","HTN  4,8/20 rudá",null,"Nasekaná smršťovací trubice 4,8/2,4mm rudá / 20mm","1000ks",14.696549650956946,{"$f":"F3952*(1-Elteq!$F$9)","v":14.696549650956946},""]
["TECHNIK","HTN  4,8/20 transp",null,"Nasekaná smršťovací trubice 4,8/2,4mm transparentní / 20mm","1000ks",14.696549650956946,{"$f":"F3953*(1-Elteq!$F$9)","v":14.696549650956946},""]
["TECHNIK","HTN  4,8/20 zelená",null,"Nasekaná smršťovací trubice 4,8/2,4mm zelená / 20mm","1000ks",14.696549650956946,{"$f":"F3954*(1-Elteq!$F$9)","v":14.696549650956946},""]
["TECHNIK","HTN  4,8/20 žlutá",null,"Nasekaná smršťovací trubice 4,8/2,4mm žlutá / 20mm","1000ks",14.696549650956946,{"$f":"F3955*(1-Elteq!$F$9)","v":14.696549650956946},""]
["TECHNIK","HTN  4,8/30 bílá",null,"Nasekaná smršťovací trubice 4,8/2,4mm bílá / 30mm","1000ks",18.259349566340447,{"$f":"F3956*(1-Elteq!$F$9)","v":18.259349566340447},""]
["TECHNIK","HTN  4,8/30 černá",null,"Nasekaná smršťovací trubice 4,8/2,4mm černá / 30mm","1000ks",18.259349566340447,{"$f":"F3957*(1-Elteq!$F$9)","v":18.259349566340447},"8591735045944"]
["TECHNIK","HTN  4,8/30 hnědá",null,"Nasekaná smršťovací trubice 4,8/2,4mm hnědá / 30mm","1000ks",18.259349566340447,{"$f":"F3958*(1-Elteq!$F$9)","v":18.259349566340447},""]
["TECHNIK","HTN  4,8/30 modrá",null,"Nasekaná smršťovací trubice 4,8/2,4mm modrá / 30mm","1000ks",18.259349566340447,{"$f":"F3959*(1-Elteq!$F$9)","v":18.259349566340447},""]
["TECHNIK","HTN  4,8/30 rudá",null,"Nasekaná smršťovací trubice 4,8/2,4mm rudá / 30mm","1000ks",18.259349566340447,{"$f":"F3960*(1-Elteq!$F$9)","v":18.259349566340447},""]
["TECHNIK","HTN  4,8/30 šedá",null,"Nasekaná smršťovací trubice 4,8/2,4mm šedá / 30mm","1000ks",18.259349566340447,{"$f":"F3961*(1-Elteq!$F$9)","v":18.259349566340447},""]
["TECHNIK","HTN  4,8/30 transp",null,"Nasekaná smršťovací trubice 4,8/2,4mm transparentní / 30mm","1000ks",18.259349566340447,{"$f":"F3962*(1-Elteq!$F$9)","v":18.259349566340447},"8591735051426"]
["TECHNIK","HTN  4,8/30 žlutá",null,"Nasekaná smršťovací trubice 4,8/2,4mm žlutá / 30mm","1000ks",18.259349566340447,{"$f":"F3963*(1-Elteq!$F$9)","v":18.259349566340447},""]
["TECHNIK","HTN  4,8/30 žz",null,"Nasekaná smršťovací trubice 4,8/2,4mm žluto-zelená / 30mm","1000ks",23.158199449992765,{"$f":"F3964*(1-Elteq!$F$9)","v":23.158199449992765},""]
["TECHNIK","HTN  6,4/20 bílá",null,"Nasekaná smršťovací trubice 6,4/3,2mm bílá / 20mm","1000ks",16.03259961922576,{"$f":"F3965*(1-Elteq!$F$9)","v":16.03259961922576},""]
["TECHNIK","HTN  6,4/20 černá",null,"Nasekaná smršťovací trubice 6,4/3,2mm černá / 20mm","1000ks",16.03259961922576,{"$f":"F3966*(1-Elteq!$F$9)","v":16.03259961922576},""]
["TECHNIK","HTN  6,4/20 modrá",null,"Nasekaná smršťovací trubice 6,4/3,2mm modrá / 20mm","1000ks",16.03259961922576,{"$f":"F3967*(1-Elteq!$F$9)","v":16.03259961922576},""]
["TECHNIK","HTN  6,4/20 rudá",null,"Nasekaná smršťovací trubice 6,4/3,2mm rudá / 20mm","1000ks",16.03259961922576,{"$f":"F3968*(1-Elteq!$F$9)","v":16.03259961922576},""]
["TECHNIK","HTN  6,4/20 zelená",null,"Nasekaná smršťovací trubice 6,4/3,2mm zelená/ 20mm","1000ks",16.03259961922576,{"$f":"F3969*(1-Elteq!$F$9)","v":16.03259961922576},""]
["TECHNIK","HTN  6,4/20 žlutá",null,"Nasekaná smršťovací trubice 6,4/3,2mm žlutá / 20mm","1000ks",16.03259961922576,{"$f":"F3970*(1-Elteq!$F$9)","v":16.03259961922576},""]
["TECHNIK","HTN  6,4/30 bílá",null,"Nasekaná smršťovací trubice 6,4/3,2mm bílá / 30mm","1000ks",20.931449502878074,{"$f":"F3971*(1-Elteq!$F$9)","v":20.931449502878074},""]
["TECHNIK","HTN  6,4/30 černá",null,"Nasekaná smršťovací trubice 6,4/3,2mm černá / 30mm","1000ks",20.931449502878074,{"$f":"F3972*(1-Elteq!$F$9)","v":20.931449502878074},"8591735045951"]
["TECHNIK","HTN  6,4/30 modrá",null,"Nasekaná smršťovací trubice 6,4/3,2mm modrá / 30mm","1000ks",20.931449502878074,{"$f":"F3973*(1-Elteq!$F$9)","v":20.931449502878074},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"HTN  6,4/30 rudá",null,"Nasekaná smršťovací trubice 6,4/3,2mm rudá / 30mm","1000ks",20.931449502878074,{"$f":"F3974*(1-Elteq!$F$9)","v":20.931449502878074},""]
["TECHNIK","HTN  6,4/30 šedá",null,"Nasekaná smršťovací trubice 6,4/3,2mm šedá / 30mm","1000ks",20.931449502878074,{"$f":"F3975*(1-Elteq!$F$9)","v":20.931449502878074},""]
["TECHNIK","HTN  6,4/30 transp",null,"Nasekaná smršťovací trubice 6,4/3,2mm transparentní / 30mm","1000ks",20.931449502878074,{"$f":"F3976*(1-Elteq!$F$9)","v":20.931449502878074},"8591735051419"]
["TECHNIK","HTN  6,4/30 žlutá",null,"Nasekaná smršťovací trubice 6,4/3,2mm žlutá / 30mm","1000ks",20.931449502878074,{"$f":"F3977*(1-Elteq!$F$9)","v":20.931449502878074},""]
["TECHNIK","HTN  6,4/30 žz",null,"Nasekaná smršťovací trubice 6,4/3,2mm žluto-zelená / 30mm","1000ks",24.494249418261575,{"$f":"F3978*(1-Elteq!$F$9)","v":24.494249418261575},""]
["TECHNIK","HTN  9,5/20 bílá",null,"Nasekaná smršťovací trubice 9,5/4,8mm bílá / 20mm","1000ks",18.259349566340447,{"$f":"F3979*(1-Elteq!$F$9)","v":18.259349566340447},""]
["TECHNIK","HTN  9,5/20 černá",null,"Nasekaná smršťovací trubice 9,5/4,8mm černá / 20mm","1000ks",18.259349566340447,{"$f":"F3980*(1-Elteq!$F$9)","v":18.259349566340447},""]
["TECHNIK","HTN  9,5/20 modrá",null,"Nasekaná smršťovací trubice 9,5/4,8mm modrá / 20mm","1000ks",18.259349566340447,{"$f":"F3981*(1-Elteq!$F$9)","v":18.259349566340447},""]
["TECHNIK","HTN  9,5/20 rudá",null,"Nasekaná smršťovací trubice 9,5/4,8mm rudá / 20mm","1000ks",18.259349566340447,{"$f":"F3982*(1-Elteq!$F$9)","v":18.259349566340447},""]
["TECHNIK","HTN  9,5/20 zelená",null,"Nasekaná smršťovací trubice 9,5/4,8mm zelená/ 20mm","1000ks",18.259349566340447,{"$f":"F3983*(1-Elteq!$F$9)","v":18.259349566340447},""]
["TECHNIK","HTN  9,5/20 žlutá",null,"Nasekaná smršťovací trubice 9,5/4,8mm žlutá / 20mm","1000ks",18.259349566340447,{"$f":"F3984*(1-Elteq!$F$9)","v":18.259349566340447},""]
["TECHNIK","HTN  9,5/30 černá",null,"Nasekaná smršťovací trubice 9,5/4,8mm černá / 30mm","1000ks",24.494249418261575,{"$f":"F3985*(1-Elteq!$F$9)","v":24.494249418261575},"8591735051402"]
["TECHNIK","HTN  9,5/30 modrá",null,"Nasekaná smršťovací trubice 9,5/4,8mm modrá / 30mm","1000ks",24.494249418261575,{"$f":"F3986*(1-Elteq!$F$9)","v":24.494249418261575},""]
["TECHNIK","HTN  9,5/30 rudá",null,"Nasekaná smršťovací trubice 9,5/4,8mm rudá / 30mm","1000ks",24.494249418261575,{"$f":"F3987*(1-Elteq!$F$9)","v":24.494249418261575},""]
["TECHNIK","HTN  9,5/30 šedá",null,"Nasekaná smršťovací trubice 9,5/4,8mm šedá / 30mm","1000ks",24.494249418261575,{"$f":"F3988*(1-Elteq!$F$9)","v":24.494249418261575},""]
["TECHNIK","HTN  9,5/30 transp",null,"Nasekaná smršťovací trubice 9,5/4,8mm transparentní / 30mm","1000ks",24.494249418261575,{"$f":"F3989*(1-Elteq!$F$9)","v":24.494249418261575},"8591735051396"]
["TECHNIK","3HTI  1,5 černá",null,"Smršťovací trubice 3:1 samozhášivá, bezhalogenová, průměr 1,5/0,5mm UL černá (po 10m)","1m",0.33772374197906113,{"$f":"F3990*(1-Elteq!$F$9)","v":0.33772374197906113},"8591735046088"]
["TECHNIK","3HTI  1,5 žz",null,"Smršťovací trubice 3:1 samozhášivá, průměr 1,5/0,5mm žluto-zelená","1m",0.37854749100949708,{"$f":"F3991*(1-Elteq!$F$9)","v":0.37854749100949708},"8591735047733"]
["TECHNIK","3HTI  3,0 bílá",null,"Smršťovací trubice 3:1 samozhášivá, bezhalogenová, průměr 3,0/1,0mm bílá (po 10m)","1m",0.52328623757195181,{"$f":"F3992*(1-Elteq!$F$9)","v":0.52328623757195181},"8591735039813"]
["TECHNIK","3HTI  3,0 černá",null,"Smršťovací trubice 3:1 samozhášivá, bezhalogenová, průměr 3,0/1,0mm černá (po 10m)","1m",0.52328623757195181,{"$f":"F3993*(1-Elteq!$F$9)","v":0.52328623757195181},"8591735046095"]
["TECHNIK","3HTI  3,0 žlutá",null,"Smršťovací trubice 3:1 samozhášivá, bezhalogenová, průměr 3,0/1,0mm žlutá (po 10m)","1m",0.52328623757195181,{"$f":"F3994*(1-Elteq!$F$9)","v":0.52328623757195181},"8591735039837"]
["TECHNIK","3HTI  4,5 černá",null,"Smršťovací trubice 3:1 samozhášivá, bezhalogenová, průměr 4,5/1,5mm černá (po 10m)","1m",0.52328623757195181,{"$f":"F3995*(1-Elteq!$F$9)","v":0.52328623757195181},"8591735046101"]
["TECHNIK","3HTI  6,0 bílá",null,"Smršťovací trubice 3:1 samozhášivá, průměr 6,0/2,0mm bílá","1m",0.76080623193085195,{"$f":"F3996*(1-Elteq!$F$9)","v":0.76080623193085195},"8591735039851"]
["TECHNIK","3HTI  6,0 černá",null,"Smršťovací trubice 3:1 samozhášivá, bezhalogenová, průměr 6,0/2,0mm černá (po 10m)","1m",0.76080623193085195,{"$f":"F3997*(1-Elteq!$F$9)","v":0.76080623193085195},"8591735046118"]
["TECHNIK","3HTI  6,0 žlutá",null,"Smršťovací trubice 3:1 samozhášivá, průměr 6,0/2,0mm žlutá","1m",0.76080623193085195,{"$f":"F3998*(1-Elteq!$F$9)","v":0.76080623193085195},"8591735039875"]
["TECHNIK","3HTI  9,0 černá",null,"Smršťovací trubice 3:1 samozhášivá, bezhalogenová, průměr 9,0/3,0mm černá (po 10m)","1m",1.1504874726759224,{"$f":"F3999*(1-Elteq!$F$9)","v":1.1504874726759224},"8591735046132"]
["TECHNIK","3HTI 12,0 černá",null,"Smršťovací trubice 3:1 samozhášivá, bezhalogenová, průměr 12,0/4,0mm černá (po 10m)","1m",1.3731624673873914,{"$f":"F4000*(1-Elteq!$F$9)","v":1.3731624673873914},"8591735046149"]
["TECHNIK","3HTI 18,0 černá",null,"Smršťovací trubice 3:1 samozhášivá, bezhalogenová, průměr 18,0/6,0mm černá (po 10m)","1m",2.2081936975553997,{"$f":"F4001*(1-Elteq!$F$9)","v":2.2081936975553997},"8591735046156"]
["TECHNIK","3HTI 24,0 černá",null,"Smršťovací trubice 3:1 samozhášivá, průměr 24,0/8,0mm černá","1m",4.00814990480644,{"$f":"F4002*(1-Elteq!$F$9)","v":4.00814990480644},"8591735046163"]
["TECHNIK","3HTI 39,0 černá",null,"Smršťovací trubice 3:1 samozhášivá, průměr 39,0/13,0mm černá","1m",6.4946873457511751,{"$f":"F4003*(1-Elteq!$F$9)","v":6.4946873457511751},"8591735046170"]
["TECHNIK","HTI  1,2 bílá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,2/0,6mm UL bílá (po 10m)","1m",0.25978749383004701,{"$f":"F4004*(1-Elteq!$F$9)","v":0.25978749383004701},"8591735042493"]
["TECHNIK","HTI  1,2 černá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,2/0,6mm UL černá (po 10m)","1m",0.25978749383004701,{"$f":"F4005*(1-Elteq!$F$9)","v":0.25978749383004701},"8591735042509"]
["TECHNIK","HTI  1,2 modrá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,2/0,6mm UL modrá (po 10m)","1m",0.25978749383004701,{"$f":"F4006*(1-Elteq!$F$9)","v":0.25978749383004701},"8591735042516"]
["TECHNIK","HTI  1,2 rudá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,2/0,6mm UL rudá (po 10m)","1m",0.25978749383004701,{"$f":"F4007*(1-Elteq!$F$9)","v":0.25978749383004701},"8591735042523"]
["TECHNIK","HTI  1,2 transp",null,"Smršťovací trubice 2:1 tenkostěnná, bezhalogenová, průměr 1,2/0,6mm transparentní (po 10m)","1m",0.25978749383004701,{"$f":"F4008*(1-Elteq!$F$9)","v":0.25978749383004701},"8591735042530"]
["TECHNIK","HTI  1,2 žlutá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,2/0,6mm UL žlutá (po 10m)","1m",0.25978749383004701,{"$f":"F4009*(1-Elteq!$F$9)","v":0.25978749383004701},"8591735042547"]
["TECHNIK","HTI  1,6 bílá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,6/0,8mm UL bílá (po 10m)","1m",0.2783437433893361,{"$f":"F4010*(1-Elteq!$F$9)","v":0.2783437433893361},"8591735043018"]
["TECHNIK","HTI  1,6 černá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,6/0,8mm UL černá (po 10m)","1m",0.2783437433893361,{"$f":"F4011*(1-Elteq!$F$9)","v":0.2783437433893361},"8591735040512"]
["TECHNIK","HTI  1,6 modrá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,6/0,8mm UL modrá (po 10m)","1m",0.2783437433893361,{"$f":"F4012*(1-Elteq!$F$9)","v":0.2783437433893361},"8591735043025"]
["TECHNIK","HTI  1,6 rudá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,6/0,8mm UL rudá (po 10m)","1m",0.2783437433893361,{"$f":"F4013*(1-Elteq!$F$9)","v":0.2783437433893361},"8591735043049"]
["TECHNIK","HTI  1,6 šedá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,6/0,8mm UL šedá (po 10m)","1m",0.2783437433893361,{"$f":"F4014*(1-Elteq!$F$9)","v":0.2783437433893361},"8591735043094"]
["TECHNIK","HTI  1,6 transp",null,"Smršťovací trubice 2:1 tenkostěnná, bezhalogenová, průměr 1,6/0,8mm transparentní (po 10m)","1m",0.2783437433893361,{"$f":"F4015*(1-Elteq!$F$9)","v":0.2783437433893361},"8591735043100"]
["TECHNIK","HTI  1,6 žlutá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,6/0,8mm UL žlutá (po 10m)","1m",0.2783437433893361,{"$f":"F4016*(1-Elteq!$F$9)","v":0.2783437433893361},"8591735043117"]
["TECHNIK","HTI  1,6 žz",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,6/0,8mm UL žluto-zelená (po 10m)","1m",0.33401249206720329,{"$f":"F4017*(1-Elteq!$F$9)","v":0.33401249206720329},"8591735043124"]
["TECHNIK","HTI  2,4 bílá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm UL bílá (po 10m)","1m",0.29689999294862518,{"$f":"F4018*(1-Elteq!$F$9)","v":0.29689999294862518},"8591735043155"]
["TECHNIK","HTI  2,4 černá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm UL černá  (po 10m)","1m",0.29689999294862518,{"$f":"F4019*(1-Elteq!$F$9)","v":0.29689999294862518},"8591735043162"]
["TECHNIK","HTI  2,4 hnědá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm UL hnědá (po 10m)","1m",0.29689999294862518,{"$f":"F4020*(1-Elteq!$F$9)","v":0.29689999294862518},"8591735053956"]
["TECHNIK","HTI  2,4 modrá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm UL modrá (po 10m)","1m",0.29689999294862518,{"$f":"F4021*(1-Elteq!$F$9)","v":0.29689999294862518},"8591735043179"]
["TECHNIK","HTI  2,4 oranžová",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm UL oranžová (po 10m)","1m",0.29689999294862518,{"$f":"F4022*(1-Elteq!$F$9)","v":0.29689999294862518},"8591735053932"]
["TECHNIK","HTI  2,4 rudá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm UL rudá (po 10m)","1m",0.29689999294862518,{"$f":"F4023*(1-Elteq!$F$9)","v":0.29689999294862518},"8591735043193"]
["TECHNIK","HTI  2,4 šedá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm UL šedá (po 10m)","1m",0.29689999294862518,{"$f":"F4024*(1-Elteq!$F$9)","v":0.29689999294862518},"8591735043308"]
["TECHNIK","HTI  2,4 transp",null,"Smršťovací trubice 2:1 tenkostěnná, bezhalogenová, průměr 2,4/1,2mm transparentní (po 10m)","1m",0.29689999294862518,{"$f":"F4025*(1-Elteq!$F$9)","v":0.29689999294862518},"8591735043292"]
["TECHNIK","HTI  2,4 zelená",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm UL zelená (po 10m)","1m",0.29689999294862518,{"$f":"F4026*(1-Elteq!$F$9)","v":0.29689999294862518},"8591735043285"]
["TECHNIK","HTI  2,4 žlutá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm UL žlutá (po 10m)","1m",0.29689999294862518,{"$f":"F4027*(1-Elteq!$F$9)","v":0.29689999294862518},"8591735043278"]
["TECHNIK","HTI  2,4 žz",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm UL žluto-zelená (po 10m)","1m",0.35256874162649238,{"$f":"F4028*(1-Elteq!$F$9)","v":0.35256874162649238},"8591735043254"]
["TECHNIK","HTI  3,2 bílá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm UL bílá (po 10m)","1m",0.31545624250791426,{"$f":"F4029*(1-Elteq!$F$9)","v":0.31545624250791426},"8591735043339"]
["TECHNIK","HTI  3,2 černá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm UL černá (po 10m)","1m",0.31545624250791426,{"$f":"F4030*(1-Elteq!$F$9)","v":0.31545624250791426},"8591735043353"]
["TECHNIK","HTI  3,2 hnědá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm UL hnědá (po 10m)","1m",0.31545624250791426,{"$f":"F4031*(1-Elteq!$F$9)","v":0.31545624250791426},"8591735043360"]
["TECHNIK","HTI  3,2 modrá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm UL modrá (po 10m)","1m",0.31545624250791426,{"$f":"F4032*(1-Elteq!$F$9)","v":0.31545624250791426},"8591735043452"]
["TECHNIK","HTI  3,2 oranžová",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm UL oranžová (po 10m)","1m",0.31545624250791426,{"$f":"F4033*(1-Elteq!$F$9)","v":0.31545624250791426},"8591735053901"]
["TECHNIK","HTI  3,2 rudá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm UL rudá (po 10m)","1m",0.31545624250791426,{"$f":"F4034*(1-Elteq!$F$9)","v":0.31545624250791426},"8591735043469"]
["TECHNIK","HTI  3,2 šedá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm UL šedá (po 10m)","1m",0.31545624250791426,{"$f":"F4035*(1-Elteq!$F$9)","v":0.31545624250791426},"8591735043377"]
["TECHNIK","HTI  3,2 transp",null,"Smršťovací trubice 2:1 tenkostěnná, bezhalogenová, průměr 3,2/1,6mm transparentní (po 10m)","1m",0.31545624250791426,{"$f":"F4036*(1-Elteq!$F$9)","v":0.31545624250791426},"8591735043476"]
["TECHNIK","HTI  3,2 zelená",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm UL zelená (po 10m)","1m",0.31545624250791426,{"$f":"F4037*(1-Elteq!$F$9)","v":0.31545624250791426},"8591735053918"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"HTI  3,2 žlutá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm UL žlutá (po 10m)","1m",0.31545624250791426,{"$f":"F4038*(1-Elteq!$F$9)","v":0.31545624250791426},"8591735037925"]
["TECHNIK","HTI  3,2 žz",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm UL žluto-zelená (po 10m)","1m",0.37112499118578146,{"$f":"F4039*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735043483"]
["TECHNIK","HTI  4,0 černá",null,"Smršťovací trubice 4:1 samozhášivá, bezhalogenová, průměr 4,0/1,0mm černá","1m",0.57524373633796122,{"$f":"F4040*(1-Elteq!$F$9)","v":0.57524373633796122},"8591735043315"]
["TECHNIK","HTI  4,8 bílá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm UL bílá (po 10m)","1m",0.37112499118578146,{"$f":"F4041*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735044046"]
["TECHNIK","HTI  4,8 černá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm UL černá (po 10m)","1m",0.37112499118578146,{"$f":"F4042*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735043964"]
["TECHNIK","HTI  4,8 fialová",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm UL fialová (po 10m)","1m",0.37112499118578146,{"$f":"F4043*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735056599"]
["TECHNIK","HTI  4,8 hnědá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm UL hnědá (po 10m)","1m",0.37112499118578146,{"$f":"F4044*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735044053"]
["TECHNIK","HTI  4,8 modrá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm UL modrá (po 10m)","1m",0.37112499118578146,{"$f":"F4045*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735043940"]
["TECHNIK","HTI  4,8 rudá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm UL rudá (po 10m)","1m",0.37112499118578146,{"$f":"F4046*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735043995"]
["TECHNIK","HTI  4,8 šedá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm UL šedá (po 10m)","1m",0.37112499118578146,{"$f":"F4047*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735044060"]
["TECHNIK","HTI  4,8 transp",null,"Smršťovací trubice 2:1 tenkostěnná, bezhalogenová, průměr 4,8/2,4mm transparentní (po 10m)","1m",0.37112499118578146,{"$f":"F4048*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735044015"]
["TECHNIK","HTI  4,8 zelená",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm UL zelená (po 10m)","1m",0.37112499118578146,{"$f":"F4049*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735044077"]
["TECHNIK","HTI  4,8 žlutá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm UL žlutá (po 10m)","1m",0.37112499118578146,{"$f":"F4050*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735043933"]
["TECHNIK","HTI  4,8 žz",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm UL žluto-zelená (po 10m)","1m",0.40823749030435963,{"$f":"F4051*(1-Elteq!$F$9)","v":0.40823749030435963},"8591735044039"]
["TECHNIK","HTI  6,4 bílá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 6,4/3,2mm UL bílá (po 10m)","1m",0.44534998942293774,{"$f":"F4052*(1-Elteq!$F$9)","v":0.44534998942293774},"8591735044091"]
["TECHNIK","HTI  6,4 černá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 6,4/3,2mm UL černá (po 10m)","1m",0.44534998942293774,{"$f":"F4053*(1-Elteq!$F$9)","v":0.44534998942293774},"8591735038007"]
["TECHNIK","HTI  6,4 hnědá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 6,4/3,2mm UL hnědá (po 10m)","1m",0.44534998942293774,{"$f":"F4054*(1-Elteq!$F$9)","v":0.44534998942293774},"8591735044114"]
["TECHNIK","HTI  6,4 modrá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 6,4/3,2mm UL modrá (po 10m)","1m",0.44534998942293774,{"$f":"F4055*(1-Elteq!$F$9)","v":0.44534998942293774},"8591735044121"]
["TECHNIK","HTI  6,4 rudá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 6,4/3,2mm UL červená (po 10m)","1m",0.44534998942293774,{"$f":"F4056*(1-Elteq!$F$9)","v":0.44534998942293774},"8591735044138"]
["TECHNIK","HTI  6,4 šedá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 6,4/3,2mm UL šedá (po 10m)","1m",0.44534998942293774,{"$f":"F4057*(1-Elteq!$F$9)","v":0.44534998942293774},"8591735044145"]
["TECHNIK","HTI  6,4 transp",null,"Smršťovací trubice 2:1 tenkostěnná, bezhalogenová, průměr 6,4/3,2mm transparentní (po 10m)","1m",0.44534998942293774,{"$f":"F4058*(1-Elteq!$F$9)","v":0.44534998942293774},"8591735044169"]
["TECHNIK","HTI  6,4 zelená",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 6,4/3,2mm UL zelená (po 10m)","1m",0.44534998942293774,{"$f":"F4059*(1-Elteq!$F$9)","v":0.44534998942293774},"8591735044176"]
["TECHNIK","HTI  6,4 žlutá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 6,4/3,2mm UL žlutá (po 10m)","1m",0.44534998942293774,{"$f":"F4060*(1-Elteq!$F$9)","v":0.44534998942293774},"8591735044206"]
["TECHNIK","HTI  6,4 žz",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 6,4/3,2mm UL žluto-zelená (po 10m)","1m",0.53813123721938316,{"$f":"F4061*(1-Elteq!$F$9)","v":0.53813123721938316},"8591735044183"]
["TECHNIK","HTI  8,0 černá",null,"Smršťovací trubice samozhášivá, průměr 8,0/2,0mm černá","1m",0.81647498060871926,{"$f":"F4062*(1-Elteq!$F$9)","v":0.81647498060871926},"8591735044237"]
["TECHNIK","HTI  9,5 bílá",null,"Smršťovací trubice samozhášivá, průměr 9,5/4,8mm bílá","1m",0.55668748677867219,{"$f":"F4063*(1-Elteq!$F$9)","v":0.55668748677867219},"8591735044367"]
["TECHNIK","HTI  9,5 černá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 9,5/4,8mm UL černá (po 10m)","1m",0.55668748677867219,{"$f":"F4064*(1-Elteq!$F$9)","v":0.55668748677867219},"8591735044268"]
["TECHNIK","HTI  9,5 modrá",null,"Smršťovací trubice samozhášivá, průměr 9,5/4,8mm modrá","1m",0.55668748677867219,{"$f":"F4065*(1-Elteq!$F$9)","v":0.55668748677867219},"8591735044275"]
["TECHNIK","HTI  9,5 rudá",null,"Smršťovací trubice samozhášivá, průměr 9,5/4,8mm rudá","1m",0.55668748677867219,{"$f":"F4066*(1-Elteq!$F$9)","v":0.55668748677867219},"8591735044299"]
["TECHNIK","HTI  9,5 šedá",null,"Smršťovací trubice samozhášivá, průměr 9,5/4,8mm šedá","1m",0.55668748677867219,{"$f":"F4067*(1-Elteq!$F$9)","v":0.55668748677867219},"8591735044220"]
["TECHNIK","HTI  9,5 transp",null,"Smršťovací trubice tenkostěnná, průměr 9,5/4,8mm transparentní","1m",0.55668748677867219,{"$f":"F4068*(1-Elteq!$F$9)","v":0.55668748677867219},"8591735044312"]
["TECHNIK","HTI  9,5 zelená",null,"Smršťovací trubice samozhášivá, průměr 9,5/4,8mm zelená","1m",0.55668748677867219,{"$f":"F4069*(1-Elteq!$F$9)","v":0.55668748677867219},"8591735044374"]
["TECHNIK","HTI  9,5 žlutá",null,"Smršťovací trubice samozhášivá, průměr 9,5/4,8mm žlutá","1m",0.55668748677867219,{"$f":"F4070*(1-Elteq!$F$9)","v":0.55668748677867219},"8591735044381"]
["TECHNIK","HTI  9,5 žz",null,"Smršťovací trubice samozhášivá, průměr 9,5/4,8mm žluto-zelená","1m",0.70513748325298475,{"$f":"F4071*(1-Elteq!$F$9)","v":0.70513748325298475},"8591735044343"]
["TECHNIK","HTI 12,7 bílá",null,"Smršťovací trubice samozhášivá 12,7/6,4mm bílá","1m",0.66802498413440659,{"$f":"F4072*(1-Elteq!$F$9)","v":0.66802498413440659},"8591735044510"]
["TECHNIK","HTI 12,7 černá",null,"Smršťovací trubice samozhášivá 12,7/6,4mm černá","1m",0.66802498413440659,{"$f":"F4073*(1-Elteq!$F$9)","v":0.66802498413440659},"8591735038014"]
["TECHNIK","HTI 12,7 modrá",null,"Smršťovací trubice samozhášivá 12,7/6,4mm modrá","1m",0.66802498413440659,{"$f":"F4074*(1-Elteq!$F$9)","v":0.66802498413440659},"8591735044480"]
["TECHNIK","HTI 12,7 oranžová",null,"Smršťovací trubice samozhášivá 12,7/6,4mm oranžová","1m",0.66802498413440659,{"$f":"F4075*(1-Elteq!$F$9)","v":0.66802498413440659},"8591735056629"]
["TECHNIK","HTI 12,7 rudá",null,"Smršťovací trubice samozhášivá 12,7/6,4mm rudá","1m",0.66802498413440659,{"$f":"F4076*(1-Elteq!$F$9)","v":0.66802498413440659},"8591735044466"]
["TECHNIK","HTI 12,7 šedá",null,"Smršťovací trubice samozhášivá 12,7/6,4mm šedá","1m",0.66802498413440659,{"$f":"F4077*(1-Elteq!$F$9)","v":0.66802498413440659},"8591735044503"]
["TECHNIK","HTI 12,7 transp",null,"Smršťovací trubice tenkostěnná 12,7/6,4mm transparentní","1m",0.66802498413440659,{"$f":"F4078*(1-Elteq!$F$9)","v":0.66802498413440659},"8591735044435"]
["TECHNIK","HTI 12,7 žlutá",null,"Smršťovací trubice samozhášivá 12,7/6,4mm žlutá","1m",0.66802498413440659,{"$f":"F4079*(1-Elteq!$F$9)","v":0.66802498413440659},"8591735044398"]
["TECHNIK","HTI 12,7 žz",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 12,7/6,4mm žluto-zelená (po 10m)","1m",1.2247124709130788,{"$f":"F4080*(1-Elteq!$F$9)","v":1.2247124709130788},"8591735044404"]
["TECHNIK","HTI 16,0 černá",null,"Smršťovací trubice samozhášivá, průměr 16/8mm černá","1m",1.2247124709130788,{"$f":"F4081*(1-Elteq!$F$9)","v":1.2247124709130788},"8591735049614"]
["TECHNIK","HTI 19,0 bílá",null,"Smršťovací trubice samozhášivá 19/9,5mm bílá","1m",1.3174937187095241,{"$f":"F4082*(1-Elteq!$F$9)","v":1.3174937187095241},"8591735044534"]
["TECHNIK","HTI 19,0 černá",null,"Smršťovací trubice samozhášivá 19/9,5mm černá","1m",1.3174937187095241,{"$f":"F4083*(1-Elteq!$F$9)","v":1.3174937187095241},"8591735033255"]
["TECHNIK","HTI 19,0 modrá",null,"Smršťovací trubice samozhášivá 19/9,5mm modrá","1m",1.3174937187095241,{"$f":"F4084*(1-Elteq!$F$9)","v":1.3174937187095241},"8591735033811"]
["TECHNIK","HTI 19,0 rudá",null,"Smršťovací trubice samozhášivá 19/9,5mm rudá","1m",1.3174937187095241,{"$f":"F4085*(1-Elteq!$F$9)","v":1.3174937187095241},"8591735044558"]
["TECHNIK","HTI 19,0 šedá",null,"Smršťovací trubice samozhášivá 19/9,5mm šedá","1m",1.3174937187095241,{"$f":"F4086*(1-Elteq!$F$9)","v":1.3174937187095241},"8591735044541"]
["TECHNIK","HTI 19,0 transp",null,"Smršťovací trubice tenkostěnná 19/9,5mm transparentní","1m",1.3174937187095241,{"$f":"F4087*(1-Elteq!$F$9)","v":1.3174937187095241},"8591735044572"]
["TECHNIK","HTI 19,0 žlutá",null,"Smršťovací trubice samozhášivá 19/9,5mm žlutá","1m",1.3174937187095241,{"$f":"F4088*(1-Elteq!$F$9)","v":1.3174937187095241},"8591735002176"]
["TECHNIK","HTI 19,0 žz",null,"Smršťovací trubice samozhášivá 19/9,5mm žluto-zelená","1m",1.7071749594545946,{"$f":"F4089*(1-Elteq!$F$9)","v":1.7071749594545946},"8591735044602"]
["TECHNIK","HTI 25,4 bílá",null,"Smršťovací trubice samozhášivá 25,4/12,7mm bílá","1m",1.8185124568103292,{"$f":"F4090*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735044640"]
["TECHNIK","HTI 25,4 černá",null,"Smršťovací trubice samozhášivá 25,4/12,7mm černá","1m",1.8185124568103292,{"$f":"F4091*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735044633"]
["TECHNIK","HTI 25,4 modrá",null,"Smršťovací trubice samozhášivá 25,4/12,7mm modrá","1m",1.8185124568103292,{"$f":"F4092*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735044657"]
["TECHNIK","HTI 25,4 rudá",null,"Smršťovací trubice samozhášivá 25,4/12,7mm rudá","1m",1.8185124568103292,{"$f":"F4093*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735044664"]
["TECHNIK","HTI 25,4 šedá",null,"Smršťovací trubice samozhášivá 25,4/12,7mm šedá","1m",1.8185124568103292,{"$f":"F4094*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735044671"]
["TECHNIK","HTI 25,4 transp",null,"Smršťovací trubice tenkostěnná 25,4/12,7mm transparentní","1m",1.8185124568103292,{"$f":"F4095*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735044688"]
["TECHNIK","HTI 25,4 žlutá",null,"Smršťovací trubice samozhášivá 25,4/12,7mm žlutá","1m",1.8185124568103292,{"$f":"F4096*(1-Elteq!$F$9)","v":1.8185124568103292},"8591735054403"]
["TECHNIK","HTI 25,4 žz",null,"Smršťovací trubice samozhášivá 25,4/12,7mm žluto-zelená","1m",1.8556249559289073,{"$f":"F4097*(1-Elteq!$F$9)","v":1.8556249559289073},"8591735044695"]
["TECHNIK","HTI 30,0 černá",null,"Smršťovací trubice samozhášivá 30/15mm černá","1m",2.4865374409447356,{"$f":"F4098*(1-Elteq!$F$9)","v":2.4865374409447356},"8591735049621"]
["TECHNIK","HTI 38,0 bílá",null,"Smršťovací trubice samozhášivá 38,0/19,0mm bílá","1m",3.0061124286048297,{"$f":"F4099*(1-Elteq!$F$9)","v":3.0061124286048297},"8591735044701"]
["TECHNIK","HTI 38,0 černá",null,"Smršťovací trubice samozhášivá 38,0/19,0mm černá","1m",3.0061124286048297,{"$f":"F4100*(1-Elteq!$F$9)","v":3.0061124286048297},"8591735044725"]
["TECHNIK","HTI 38,0 modrá",null,"Smršťovací trubice samozhášivá 38,0/19,0mm modrá","1m",3.0061124286048297,{"$f":"F4101*(1-Elteq!$F$9)","v":3.0061124286048297},"8591735044732"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"HTI 38,0 oranž",null,"Smršťovací trubice samozhášivá 38,0/19,0mm oranžová","1m",3.0061124286048297,{"$f":"F4102*(1-Elteq!$F$9)","v":3.0061124286048297},"8591735057091"]
["TECHNIK","HTI 38,0 rudá",null,"Smršťovací trubice samozhášivá 38,0/19,0mm rudá","1m",3.0061124286048297,{"$f":"F4103*(1-Elteq!$F$9)","v":3.0061124286048297},"8591735044749"]
["TECHNIK","HTI 38,0 šedá",null,"Smršťovací trubice samozhášivá 38,0/19,0mm šedá","1m",3.0061124286048297,{"$f":"F4104*(1-Elteq!$F$9)","v":3.0061124286048297},"8591735044770"]
["TECHNIK","HTI 38,0 transp",null,"Smršťovací trubice tenkostěnná 38,0/19,0mm transparentní","1m",3.0061124286048297,{"$f":"F4105*(1-Elteq!$F$9)","v":3.0061124286048297},"8591735044756"]
["TECHNIK","HTI 38,0 žlutá",null,"Smršťovací trubice tenkostěnná 38,0/19,0mm žlutá","1m",3.0061124286048297,{"$f":"F4106*(1-Elteq!$F$9)","v":3.0061124286048297},"8591735054960"]
["TECHNIK","HTI 38,0 žz",null,"Smršťovací trubice samozhášivá 38,0/19,0mm žluto-zelená","1m",3.4143499189091893,{"$f":"F4107*(1-Elteq!$F$9)","v":3.4143499189091893},"8591735044800"]
["TECHNIK","HTI 51,0 bílá",null,"Smršťovací trubice samozhášivá 50,8/25,4mm bílá","1m",5.641099866023878,{"$f":"F4108*(1-Elteq!$F$9)","v":5.641099866023878},"8591735044909"]
["TECHNIK","HTI 51,0 černá",null,"Smršťovací trubice samozhášivá 50,8/25,4mm černá","1m",5.641099866023878,{"$f":"F4109*(1-Elteq!$F$9)","v":5.641099866023878},"8591735037901"]
["TECHNIK","HTI 51,0 modrá",null,"Smršťovací trubice samozhášivá 50,8/25,4mm modrá","1m",5.641099866023878,{"$f":"F4110*(1-Elteq!$F$9)","v":5.641099866023878},"8591735044916"]
["TECHNIK","HTI 51,0 oranžová",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 50,8/25,4mm UL, oranžová","1m",5.641099866023878,{"$f":"F4111*(1-Elteq!$F$9)","v":5.641099866023878},"8591735056780"]
["TECHNIK","HTI 51,0 rudá",null,"Smršťovací trubice samozhášivá 50,8/25,4mm rudá","1m",5.641099866023878,{"$f":"F4112*(1-Elteq!$F$9)","v":5.641099866023878},"8591735044923"]
["TECHNIK","HTI 51,0 šedá",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 50,8/25,4mm šedá","1m",5.641099866023878,{"$f":"F4113*(1-Elteq!$F$9)","v":5.641099866023878},"8591735044879"]
["TECHNIK","HTI 51,0 transp",null,"Smršťovací trubice tenkostěnná 50,8/25,4mm transparentní","1m",5.641099866023878,{"$f":"F4114*(1-Elteq!$F$9)","v":5.641099866023878},"8591735042486"]
["TECHNIK","HTI 51,0 zelená",null,"Smršťovací trubice samozhášivá 50,8/25,4mm zelená","1m",5.641099866023878,{"$f":"F4115*(1-Elteq!$F$9)","v":5.641099866023878},"8591735044930"]
["TECHNIK","HTI 51,0 žz",null,"Smršťovací trubice samozhášivá 50,8/25,4mm žluto-zelená","1m",6.0864498554468156,{"$f":"F4116*(1-Elteq!$F$9)","v":6.0864498554468156},"8591735044947"]
["TECHNIK","HTI 76,2 černá",null,"Smršťovací trubice samozhášivá 76,2/38,1mm černá","1m",7.8678498131385668,{"$f":"F4117*(1-Elteq!$F$9)","v":7.8678498131385668},"8591735044954"]
["TECHNIK","HTI 76,2 rudá",null,"Smršťovací trubice samozhášivá 76,2/38,1mm rudá","1m",7.8678498131385668,{"$f":"F4118*(1-Elteq!$F$9)","v":7.8678498131385668},"8591735044978"]
["TECHNIK","HTI 76,2 šedá",null,"Smršťovací trubice samozhášivá 76,2/38,1mm šedá","1m",7.8678498131385668,{"$f":"F4119*(1-Elteq!$F$9)","v":7.8678498131385668},"8591735044985"]
["TECHNIK","HTI 76,2 transp",null,"Smršťovací trubice tenkostěnná 76,2/38,1mm transparentní","1m",7.8678498131385668,{"$f":"F4120*(1-Elteq!$F$9)","v":7.8678498131385668},"8591735045005"]
["TECHNIK","HTI 76,2 zelená",null,"Smršťovací trubice samozhášivá 76,2/38,1mm zelená","1m",10.317274754964725,{"$f":"F4121*(1-Elteq!$F$9)","v":10.317274754964725},"8591735045029"]
["TECHNIK","HTI 76,2 žz",null,"Smršťovací trubice samozhášivá 76,2/38,1mm žluto-zelená","1m",11.579099724996382,{"$f":"F4122*(1-Elteq!$F$9)","v":11.579099724996382},"8591735055011"]
["TECHNIK","HTI102,0 černá",null,"Smršťovací trubice samozhášivá 102/51mm černá","1m",9.7976997673046302,{"$f":"F4123*(1-Elteq!$F$9)","v":9.7976997673046302},"8591735042400"]
["TECHNIK","HTI102,0 modrá",null,"Smršťovací trubice samozhášivá 102/51mm modrá","1m",9.7976997673046302,{"$f":"F4124*(1-Elteq!$F$9)","v":9.7976997673046302},"8591735045050"]
["TECHNIK","HTI102,0 rudá",null,"Smršťovací trubice samozhášivá 102/51mm rudá","1m",9.7976997673046302,{"$f":"F4125*(1-Elteq!$F$9)","v":9.7976997673046302},"8591735045074"]
["TECHNIK","HTI102,0 transp",null,"Smršťovací trubice tenkostěnná 102/51mm transparentní","1m",9.7976997673046302,{"$f":"F4126*(1-Elteq!$F$9)","v":9.7976997673046302},"8591735045098"]
["TECHNIK","HTI126,0 černá",null,"Smršťovací trubice samozhášivá 126/63mm černá (cívka 15m)","1m",20.968562001996652,{"$f":"F4127*(1-Elteq!$F$9)","v":20.968562001996652},"8591735045104"]
["TECHNIK","HTI150,0 černá",null,"Smršťovací trubice samozhášivá 150/75mm černá (cívka 15m)","1m",25.9787493830047,{"$f":"F4128*(1-Elteq!$F$9)","v":25.9787493830047},"8591735045111"]
["TECHNIK","HTI200,0 černá",null,"Smršťovací trubice samozhášivá 200/100mm černá","1,22m",41.603111511926102,{"$f":"F4129*(1-Elteq!$F$9)","v":41.603111511926102},"8591735045135"]
["TECHNIK","HTI250,0 černá",null,"Smršťovací trubice samozhášivá 250/125mm černá","1,22m",54.518261205191294,{"$f":"F4130*(1-Elteq!$F$9)","v":54.518261205191294},"8591735045142"]
["TECHNIK","HTI300,0 černá",null,"Smršťovací trubice samozhášivá 300/150mm černá","1,22m",73.37141075742899,{"$f":"F4131*(1-Elteq!$F$9)","v":73.37141075742899},"8591735045159"]
["TECHNIK","HTI350,0 černá",null,"Smršťovací trubice samozhášivá 350/175mm černá","1,22m",92.113222812310951,{"$f":"F4132*(1-Elteq!$F$9)","v":92.113222812310951},"8591735045166"]
["TECHNIK","3HTI  1,5 černá R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 1,5/0,5mm černá (cívka 150m)","150m",46.205061402629795,{"$f":"F4133*(1-Elteq!$F$9)","v":46.205061402629795},"8591735039806"]
["TECHNIK","3HTI  1,5 žlutá R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 1,5/0,5mm žlutá (cívka 150m)","150m",46.205061402629795,{"$f":"F4134*(1-Elteq!$F$9)","v":46.205061402629795},"8591735047771"]
["TECHNIK","3HTI  1,5 žz R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 1,5/0,5mm žluto-zelená (cívka 150m)","150m",51.58637377482362,{"$f":"F4135*(1-Elteq!$F$9)","v":51.58637377482362},"8591735047375"]
["TECHNIK","3HTI  3,0 bílá T2",null,"Smršťovací trubice 3:1 samozhášivá, průměr 3,0/1,0mm bílá vhodná k potisku (cívka 200m)","200m",95.379122734745835,{"$f":"F4136*(1-Elteq!$F$9)","v":95.379122734745835},"8591735051013"]
["TECHNIK","3HTI  3,0 černá R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 3,0/1,0mm černá (cívka 150m)","150m",64.575748466325976,{"$f":"F4137*(1-Elteq!$F$9)","v":64.575748466325976},"8591735039820"]
["TECHNIK","3HTI  3,0 žlutá T2",null,"Smršťovací trubice 3:1 samozhášivá, průměr 3,0/1,0mm žlutá vhodná k potisku (cívka 200m)","200m",95.379122734745835,{"$f":"F4138*(1-Elteq!$F$9)","v":95.379122734745835},"8591735051099"]
["TECHNIK","3HTI  3,0 žz R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 3,0/1,0mm žluto-zelená (cívka 150m)","150m",71.998248290041602,{"$f":"F4139*(1-Elteq!$F$9)","v":71.998248290041602},"8591735047382"]
["TECHNIK","3HTI  4,5 bílá T1",null,"Smršťovací trubice 3:1 samozhášivá, průměr 4,8/1,6mm bílá vhodná k potisku (cívka 100m) plochá","100m",84.245372999172389,{"$f":"F4140*(1-Elteq!$F$9)","v":84.245372999172389},"8591735036881"]
["TECHNIK","3HTI  4,5 černá R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 4,5/1,5mm černá (cívka 75m)","75m",35.62799915383502,{"$f":"F4141*(1-Elteq!$F$9)","v":35.62799915383502},"8591735039844"]
["TECHNIK","3HTI  4,5 transp R",null,"Smršťovací trubice 3:1 tenkostěnná, průměr 4,5/1,5mm transparentní (cívka 75m)","75m",35.62799915383502,{"$f":"F4142*(1-Elteq!$F$9)","v":35.62799915383502},"8591735046675"]
["TECHNIK","3HTI  4,5 žlutá R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 4,5/1,5mm žlutá (cívka 75m)","75m",35.62799915383502,{"$f":"F4143*(1-Elteq!$F$9)","v":35.62799915383502},"8591735050986"]
["TECHNIK","3HTI  4,5 žlutá T1",null,"Smršťovací trubice 3:1 samozhášivá, průměr 4,8/1,6mm žlutá vhodná k potisku (cívka 100m) plochá","100m",84.245372999172389,{"$f":"F4144*(1-Elteq!$F$9)","v":84.245372999172389},"8591735051259"]
["TECHNIK","3HTI  4,5 žz R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 4,5/1,5mm žluto-zelená (cívka 75m)","75m",40.081499048064394,{"$f":"F4145*(1-Elteq!$F$9)","v":40.081499048064394},"8591735047115"]
["TECHNIK","3HTI  6,0 bílá T1",null,"Smršťovací trubice 3:1 samozhášivá, bezhalogenová, průměr 6,4/2,0mm bílá pro tisk (cívka100m) plochá","100m",100.94599760253256,{"$f":"F4146*(1-Elteq!$F$9)","v":100.94599760253256},"8591735041519"]
["TECHNIK","3HTI  6,0 černá R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 6,0/2,0mm černá (cívka 75m)","75m",51.21524878363784,{"$f":"F4147*(1-Elteq!$F$9)","v":51.21524878363784},"8591735039868"]
["TECHNIK","3HTI  6,0 žlutá T1",null,"Smršťovací trubice 3:1 samozhášivá, bezhalogenová, průměr 6,4/2,0mm žlutá pro tisk (cívka100) plochá","100m",100.94599760253256,{"$f":"F4148*(1-Elteq!$F$9)","v":100.94599760253256},"8591735051266"]
["TECHNIK","3HTI  6,0 žz R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 6,0/2,0mm žluto-zelená (cívka 75m)","75m",57.524373633796124,{"$f":"F4149*(1-Elteq!$F$9)","v":57.524373633796124},"8591735047122"]
["TECHNIK","3HTI  9,0 černá R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 9,0/3,0mm černá (cívka 75m)","75m",77.936248149014105,{"$f":"F4150*(1-Elteq!$F$9)","v":77.936248149014105},"8591735039882"]
["TECHNIK","3HTI  9,0 modrá R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 9,0/3,0mm modrá (cívka 75m)","75m",77.936248149014105,{"$f":"F4151*(1-Elteq!$F$9)","v":77.936248149014105},"8591735039899"]
["TECHNIK","3HTI  9,0 rudá R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 9,0/3,0mm rudá (cívka 75m)","75m",77.936248149014105,{"$f":"F4152*(1-Elteq!$F$9)","v":77.936248149014105},"8591735039905"]
["TECHNIK","3HTI  9,0 žz R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 9,0/3,0mm žluto-zelená (cívka 75m)","75m",87.214372928658648,{"$f":"F4153*(1-Elteq!$F$9)","v":87.214372928658648},"8591735047139"]
["TECHNIK","3HTI 12,0 černá R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 12,0/4,0mm černá (cívka 50m)","50m",61.977873528025505,{"$f":"F4154*(1-Elteq!$F$9)","v":61.977873528025505},"8591735039912"]
["TECHNIK","3HTI 12,0 modrá R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 12,0/4,0mm modrá (cívka 50m)","50m",61.977873528025505,{"$f":"F4155*(1-Elteq!$F$9)","v":61.977873528025505},"8591735054236"]
["TECHNIK","3HTI 12,0 žz R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 12,0/4,0mm žluto-zelená (cívka 50m)","50m",73.482748254784724,{"$f":"F4156*(1-Elteq!$F$9)","v":73.482748254784724},"8591735039929"]
["TECHNIK","3HTI 18,0 bílá R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 18,0/6,0mm bílá (cívka 30m)","30m",60.122248572096595,{"$f":"F4157*(1-Elteq!$F$9)","v":60.122248572096595},"8591735051273"]
["TECHNIK","3HTI 18,0 černá R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 18,0/6,0mm černá (cívka 30m)","30m",60.122248572096595,{"$f":"F4158*(1-Elteq!$F$9)","v":60.122248572096595},"8591735039936"]
["TECHNIK","3HTI 18,0 černá R.",null,"Smršťovací trubice 3:1 samozhášivá, průměr 18,0/6,0mm černá (cívka 50m!!!)","50m",100.203747620161,{"$f":"F4159*(1-Elteq!$F$9)","v":100.203747620161},"8591735046873"]
["TECHNIK","3HTI 18,0 rudá R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 18,0/6,0mm rudá (cívka 30m)","30m",60.122248572096595,{"$f":"F4160*(1-Elteq!$F$9)","v":60.122248572096595},"8591735046248"]
["TECHNIK","3HTI 18,0 transp R",null,"Smršťovací trubice 3:1 tenkostěnná, průměr 18,0/6,0mm transparentní (cívka 30m)","30m",60.122248572096595,{"$f":"F4161*(1-Elteq!$F$9)","v":60.122248572096595},"8591735052973"]
["TECHNIK","3HTI 18,0 žz R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 24,0/8,0mm žluto-zelená (cívka 30m)","30m",76.080623193085202,{"$f":"F4162*(1-Elteq!$F$9)","v":76.080623193085202},"8591735049294"]
["TECHNIK","3HTI 24,0 bílá R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 24,0/8,0mm bílá (cívka 30m)","30m",107.9973724350624,{"$f":"F4163*(1-Elteq!$F$9)","v":107.9973724350624},"8591735056049"]
["TECHNIK","3HTI 24,0 černá R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 24,0/8,0mm černá (cívka 30m)","30m",107.9973724350624,{"$f":"F4164*(1-Elteq!$F$9)","v":107.9973724350624},"8591735039943"]
["TECHNIK","3HTI 24,0 zelená R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 24,0/8,0mm zelená (cívka 30m)","30m",107.9973724350624,{"$f":"F4165*(1-Elteq!$F$9)","v":107.9973724350624},"8591735039950"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"3HTI 24,0 žz R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 24,0/8,0mm žluto-zelená (cívka 30m)","30m",128.03812195909461,{"$f":"F4166*(1-Elteq!$F$9)","v":128.03812195909461},"8591735039967"]
["TECHNIK","3HTI 39,0 černá R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 39,0/13,0mm černá (cívka 30m)","30m",167.00624603360166,{"$f":"F4167*(1-Elteq!$F$9)","v":167.00624603360166},"8591735039974"]
["TECHNIK","3HTI 39,0 modrá R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 39,0/13,0mm modrá (cívka 30m)","30m",167.00624603360166,{"$f":"F4168*(1-Elteq!$F$9)","v":167.00624603360166},"8591735054618"]
["TECHNIK","3HTI 39,0 rudá R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 39,0/13,0mm rudá (cívka 30m)","30m",167.00624603360166,{"$f":"F4169*(1-Elteq!$F$9)","v":167.00624603360166},"8591735054601"]
["TECHNIK","3HTI 39,0 žz R",null,"Smršťovací trubice 3:1 samozhášivá, průměr 39,0/13,0mm žlutozelená (cívka 30m)","30m",183.70687063696181,{"$f":"F4170*(1-Elteq!$F$9)","v":183.70687063696181},"8591735048693"]
["TECHNIK","HTI  1,2 bílá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,2/0,6mm UL bílá (cívka 150m)","150m",30.061124286048297,{"$f":"F4171*(1-Elteq!$F$9)","v":30.061124286048297},"8591735042479"]
["TECHNIK","HTI  1,2 černá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,2/0,6mm UL černá (cívka 150m)","150m",30.061124286048297,{"$f":"F4172*(1-Elteq!$F$9)","v":30.061124286048297},"8591735017002"]
["TECHNIK","HTI  1,2 modrá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,2/0,6mm UL modrá (cívka 150m)","150m",30.061124286048297,{"$f":"F4173*(1-Elteq!$F$9)","v":30.061124286048297},"8591735040468"]
["TECHNIK","HTI  1,2 rudá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,2/0,6mm UL rudá (cívka 150m)","150m",30.061124286048297,{"$f":"F4174*(1-Elteq!$F$9)","v":30.061124286048297},"8591735040475"]
["TECHNIK","HTI  1,2 transp R",null,"Smršťovací trubice 2:1 tenkostěnná, bezhalogenová, průměr 1,2/0,6mm transparentní (cívka 150m)","150m",30.061124286048297,{"$f":"F4175*(1-Elteq!$F$9)","v":30.061124286048297},"8591735040482"]
["TECHNIK","HTI  1,2 žlutá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,2/0,6mm UL žlutá (cívka 150m)","150m",30.061124286048297,{"$f":"F4176*(1-Elteq!$F$9)","v":30.061124286048297},"8591735040499"]
["TECHNIK","HTI  1,6 bílá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,6/0,8mm UL bílá (cívka 150m)","150m",31.174499259605643,{"$f":"F4177*(1-Elteq!$F$9)","v":31.174499259605643},"8591735040505"]
["TECHNIK","HTI  1,6 černá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,6/0,8mm UL černá (cívka 150m)","150m",31.174499259605643,{"$f":"F4178*(1-Elteq!$F$9)","v":31.174499259605643},"8591735015534"]
["TECHNIK","HTI  1,6 modrá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,6/0,8mm UL modrá (cívka 150m)","150m",31.174499259605643,{"$f":"F4179*(1-Elteq!$F$9)","v":31.174499259605643},"8591735043032"]
["TECHNIK","HTI  1,6 rudá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,6/0,8mm UL rudá (cívka 150m)","150m",31.174499259605643,{"$f":"F4180*(1-Elteq!$F$9)","v":31.174499259605643},"8591735043056"]
["TECHNIK","HTI  1,6 šedá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,6/0,8mm UL šedá (cívka 150m)","150m",31.174499259605643,{"$f":"F4181*(1-Elteq!$F$9)","v":31.174499259605643},"8591735043063"]
["TECHNIK","HTI  1,6 transp R",null,"Smršťovací trubice 2:1 tenkostěnná, bezhalogenová, průměr 1,6/0,8mm transparentní (cívka 150m)","150m",31.174499259605643,{"$f":"F4182*(1-Elteq!$F$9)","v":31.174499259605643},"8591735026950"]
["TECHNIK","HTI  1,6 žlutá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,6/0,8mm UL žlutá (cívka 150m)","150m",31.174499259605643,{"$f":"F4183*(1-Elteq!$F$9)","v":31.174499259605643},"8591735043070"]
["TECHNIK","HTI  1,6 žz R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 1,6/0,8mm UL žluto-zelená (cívka 150m)","150m",37.854749100949711,{"$f":"F4184*(1-Elteq!$F$9)","v":37.854749100949711},"8591735043087"]
["TECHNIK","HTI  2,4 bílá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm UL bílá (cívka 150m)","150m",34.514624180277679,{"$f":"F4185*(1-Elteq!$F$9)","v":34.514624180277679},"8591735029388"]
["TECHNIK","HTI  2,4 bílá T2",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm bílá pro tisk (cívka 200m)","200m",57.895498624981904,{"$f":"F4186*(1-Elteq!$F$9)","v":57.895498624981904},"8591735051297"]
["TECHNIK","HTI  2,4 bílá T3",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm bílá pro tisk (cívka30m) plochá","30m",12.247124709130787,{"$f":"F4187*(1-Elteq!$F$9)","v":12.247124709130787},"8591735045777"]
["TECHNIK","HTI  2,4 černá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm UL černá (cívka 150m)","150m",34.514624180277679,{"$f":"F4188*(1-Elteq!$F$9)","v":34.514624180277679},"8591735016944"]
["TECHNIK","HTI  2,4 hnědá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm UL hnědá (cívka 150m)","150m",34.514624180277679,{"$f":"F4189*(1-Elteq!$F$9)","v":34.514624180277679},"8591735053949"]
["TECHNIK","HTI  2,4 modrá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm UL modrá (cívka 150m)","150m",34.514624180277679,{"$f":"F4190*(1-Elteq!$F$9)","v":34.514624180277679},"8591735043186"]
["TECHNIK","HTI  2,4 oranžová R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm UL oranžová (cívka 150m)","150m",34.514624180277679,{"$f":"F4191*(1-Elteq!$F$9)","v":34.514624180277679},"8591735053925"]
["TECHNIK","HTI  2,4 rudá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm UL rudá (cívka 150m)","150m",34.514624180277679,{"$f":"F4192*(1-Elteq!$F$9)","v":34.514624180277679},"8591735043209"]
["TECHNIK","HTI  2,4 šedá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm UL šedá (cívka 150m)","150m",34.514624180277679,{"$f":"F4193*(1-Elteq!$F$9)","v":34.514624180277679},"8591735043216"]
["TECHNIK","HTI  2,4 transp R",null,"Smršťovací trubice 2:1 tenkostěnná, bezhalogenová, průměr 2,4/1,2mm transparentní (cívka 150m)","150m",34.514624180277679,{"$f":"F4194*(1-Elteq!$F$9)","v":34.514624180277679},"8591735043223"]
["TECHNIK","HTI  2,4 zelená R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm UL zelená (cívka 150m)","150m",34.514624180277679,{"$f":"F4195*(1-Elteq!$F$9)","v":34.514624180277679},"8591735043230"]
["TECHNIK","HTI  2,4 žlutá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm UL žlutá (cívka 150m)","150m",34.514624180277679,{"$f":"F4196*(1-Elteq!$F$9)","v":34.514624180277679},"8591735043247"]
["TECHNIK","HTI  2,4 žlutá T2",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm žlutá pro tisk (cívka)","200m",57.895498624981904,{"$f":"F4197*(1-Elteq!$F$9)","v":57.895498624981904},"8591735051303"]
["TECHNIK","HTI  2,4 žlutá T3",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm žlutá pro tisk (cívka30m) plochá","30m",12.247124709130787,{"$f":"F4198*(1-Elteq!$F$9)","v":12.247124709130787},"8591735045784"]
["TECHNIK","HTI  2,4 žz R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 2,4/1,2mm UL žluto-zelená (cívka 150m)","150m",40.638186534843072,{"$f":"F4199*(1-Elteq!$F$9)","v":40.638186534843072},"8591735043261"]
["TECHNIK","HTI  3,2 bílá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm UL bílá (cívka 150m)","150m",36.184686640613691,{"$f":"F4200*(1-Elteq!$F$9)","v":36.184686640613691},"8591735043346"]
["TECHNIK","HTI  3,2 bílá T1",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm bílá pro tisk (cívka100m) plochá","100m",55.29762368668144,{"$f":"F4201*(1-Elteq!$F$9)","v":55.29762368668144},"8591735051327"]
["TECHNIK","HTI  3,2 bílá T2",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm bílá pro tisk (cívka200m)","200m",64.575748466325976,{"$f":"F4202*(1-Elteq!$F$9)","v":64.575748466325976},"8591735051006"]
["TECHNIK","HTI  3,2 bílá T3",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm bílá pro tisk (cívka30m) plochá","30m",13.360499682688133,{"$f":"F4203*(1-Elteq!$F$9)","v":13.360499682688133},"8591735045791"]
["TECHNIK","HTI  3,2 černá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm UL černá (cívka 150m)","150m",36.184686640613691,{"$f":"F4204*(1-Elteq!$F$9)","v":36.184686640613691},"8591735016951"]
["TECHNIK","HTI  3,2 hnědá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm UL hnědá (cívka 150m)","150m",36.184686640613691,{"$f":"F4205*(1-Elteq!$F$9)","v":36.184686640613691},"8591735043391"]
["TECHNIK","HTI  3,2 modrá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm UL modrá (cívka 150m)","150m",36.184686640613691,{"$f":"F4206*(1-Elteq!$F$9)","v":36.184686640613691},"8591735043407"]
["TECHNIK","HTI  3,2 oranžová R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm UL oranžová (cívka 150m)","150m",36.184686640613691,{"$f":"F4207*(1-Elteq!$F$9)","v":36.184686640613691},"8591735047535"]
["TECHNIK","HTI  3,2 rudá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm UL rudá (cívka 150m)","150m",36.184686640613691,{"$f":"F4208*(1-Elteq!$F$9)","v":36.184686640613691},"8591735043414"]
["TECHNIK","HTI  3,2 šedá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm UL šedá (cívka 150m)","150m",36.184686640613691,{"$f":"F4209*(1-Elteq!$F$9)","v":36.184686640613691},"8591735043421"]
["TECHNIK","HTI  3,2 transp R",null,"Smršťovací trubice 2:1 tenkostěnná, bezhalogenová, průměr 3,2/1,6mm transparentní (cívka 150m)","150m",36.184686640613691,{"$f":"F4210*(1-Elteq!$F$9)","v":36.184686640613691},"8591735043438"]
["TECHNIK","HTI  3,2 zelená R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm UL zelená (cívka 150m)","150m",36.184686640613691,{"$f":"F4211*(1-Elteq!$F$9)","v":36.184686640613691},"8591735052539"]
["TECHNIK","HTI  3,2 žlutá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm UL žlutá (cívka 150m)","150m",36.184686640613691,{"$f":"F4212*(1-Elteq!$F$9)","v":36.184686640613691},"8591735043384"]
["TECHNIK","HTI  3,2 žlutá T1",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm žlutá pro tisk (cívka100) plochá","100m",55.29762368668144,{"$f":"F4213*(1-Elteq!$F$9)","v":55.29762368668144},"8591735051334"]
["TECHNIK","HTI  3,2 žlutá T2",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm žlutá pro tisk (cívka200)","200m",64.575748466325976,{"$f":"F4214*(1-Elteq!$F$9)","v":64.575748466325976},"8591735051082"]
["TECHNIK","HTI  3,2 žlutá T3",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm žlutá pro tisk (cívka30m) plochá","30m",13.360499682688133,{"$f":"F4215*(1-Elteq!$F$9)","v":13.360499682688133},"8591735045807"]
["TECHNIK","HTI  3,2 žz R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 3,2/1,6mm UL žluto-zelená (cívka 150m)","150m",42.864936481957756,{"$f":"F4216*(1-Elteq!$F$9)","v":42.864936481957756},"8591735043445"]
["TECHNIK","HTI  4,0 černá R",null,"Smršťovací trubice 4:1 samozhášivá, bezhalogenová, průměr 4,0/1,0mm černá (cívka 100m)","100m",51.58637377482362,{"$f":"F4217*(1-Elteq!$F$9)","v":51.58637377482362},"8591735043322"]
["TECHNIK","HTI  4,8 bílá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm UL bílá (cívka 75m)","75m",21.154124497589542,{"$f":"F4218*(1-Elteq!$F$9)","v":21.154124497589542},"8591735043957"]
["TECHNIK","HTI  4,8 bílá T1",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm bílá pro tisk (cívka100m)","100m",38.225874092135491,{"$f":"F4219*(1-Elteq!$F$9)","v":38.225874092135491},"8591735051310"]
["TECHNIK","HTI  4,8 bílá T3",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm bílá pro tisk (cívka30m) plochá","30m",14.473874656245476,{"$f":"F4220*(1-Elteq!$F$9)","v":14.473874656245476},"8591735045814"]
["TECHNIK","HTI  4,8 černá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm UL černá (cívka 75m)","75m",21.154124497589542,{"$f":"F4221*(1-Elteq!$F$9)","v":21.154124497589542},"8591735016968"]
["TECHNIK","HTI  4,8 fialová R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm UL fialová (cívka 75m)","75m",21.154124497589542,{"$f":"F4222*(1-Elteq!$F$9)","v":21.154124497589542},"8591735045975"]
["TECHNIK","HTI  4,8 hnědá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm UL hnědá (cívka 75m)","75m",21.154124497589542,{"$f":"F4223*(1-Elteq!$F$9)","v":21.154124497589542},"8591735043971"]
["TECHNIK","HTI  4,8 modrá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm UL modrá (cívka 75m)","75m",21.154124497589542,{"$f":"F4224*(1-Elteq!$F$9)","v":21.154124497589542},"8591735043988"]
["TECHNIK","HTI  4,8 oranžová R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm UL oranžová (cívka 75m)","75m",21.154124497589542,{"$f":"F4225*(1-Elteq!$F$9)","v":21.154124497589542},"8591735045982"]
["TECHNIK","HTI  4,8 rudá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm UL rudá (cívka 75m)","75m",21.154124497589542,{"$f":"F4226*(1-Elteq!$F$9)","v":21.154124497589542},"8591735038793"]
["TECHNIK","HTI  4,8 šedá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm UL šedá (cívka 75m)","75m",21.154124497589542,{"$f":"F4227*(1-Elteq!$F$9)","v":21.154124497589542},"8591735044008"]
["TECHNIK","HTI  4,8 transp R",null,"Smršťovací trubice 2:1 tenkostěnná, bezhalogenová, průměr 4,8/2,4mm transparentní (cívka 75m)","75m",21.154124497589542,{"$f":"F4228*(1-Elteq!$F$9)","v":21.154124497589542},"8591735037666"]
["TECHNIK","HTI  4,8 zelená R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm UL zekená (cívka 75m)","75m",21.154124497589542,{"$f":"F4229*(1-Elteq!$F$9)","v":21.154124497589542},"8591735042097"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"HTI  4,8 žlutá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm UL žlutá (cívka 75m)","75m",21.154124497589542,{"$f":"F4230*(1-Elteq!$F$9)","v":21.154124497589542},"8591735036706"]
["TECHNIK","HTI  4,8 žlutá T1",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm žlutá pro tisk (cívka 100m)","100m",38.225874092135491,{"$f":"F4231*(1-Elteq!$F$9)","v":38.225874092135491},"8591735051235"]
["TECHNIK","HTI  4,8 žlutá T3",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm žlutá pro tisk (cívka30m) plochá","30m",14.473874656245476,{"$f":"F4232*(1-Elteq!$F$9)","v":14.473874656245476},"8591735045821"]
["TECHNIK","HTI  4,8 žz R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 4,8/2,4mm UL žluto-zelená (cívka 75m)","75m",23.937561931482904,{"$f":"F4233*(1-Elteq!$F$9)","v":23.937561931482904},"8591735044022"]
["TECHNIK","HTI  6,4 bílá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 6,4/3,2mm UL bílá (cívka 75m)","75m",26.44265562198693,{"$f":"F4234*(1-Elteq!$F$9)","v":26.44265562198693},"8591735044084"]
["TECHNIK","HTI  6,4 bílá T1",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 6,4/3,2mm bílá pro tisk (cívka 100m)","100m",54.184248713124092,{"$f":"F4235*(1-Elteq!$F$9)","v":54.184248713124092},"8591735036874"]
["TECHNIK","HTI  6,4 bílá T3",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 6,4/3,2mm bílá pro tisk (cívka30m) plochá","30m",17.81399957691751,{"$f":"F4236*(1-Elteq!$F$9)","v":17.81399957691751},"8591735045838"]
["TECHNIK","HTI  6,4 černá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 6,4/3,2mm UL černá (cívka 75m)","75m",26.44265562198693,{"$f":"F4237*(1-Elteq!$F$9)","v":26.44265562198693},"8591735016975"]
["TECHNIK","HTI  6,4 hnědá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 6,4/3,2mm UL hnědá (cívka 75m)","75m",26.44265562198693,{"$f":"F4238*(1-Elteq!$F$9)","v":26.44265562198693},"8591735044107"]
["TECHNIK","HTI  6,4 modrá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 6,4/3,2mm UL modrá (cívka 75m)","75m",26.44265562198693,{"$f":"F4239*(1-Elteq!$F$9)","v":26.44265562198693},"8591735042431"]
["TECHNIK","HTI  6,4 rudá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 6,4/3,2mm UL červená (cívka 75m)","75m",26.44265562198693,{"$f":"F4240*(1-Elteq!$F$9)","v":26.44265562198693},"8591735042424"]
["TECHNIK","HTI  6,4 šedá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 6,4/3,2mm UL šedá (cívka 75m)","75m",26.44265562198693,{"$f":"F4241*(1-Elteq!$F$9)","v":26.44265562198693},"8591735044152"]
["TECHNIK","HTI  6,4 transp R",null,"Smršťovací trubice 2:1 tenkostěnná, bezhalogenová, průměr 6,4/3,2mm transparentní (cívka 75m)","75m",26.44265562198693,{"$f":"F4242*(1-Elteq!$F$9)","v":26.44265562198693},"8591735042448"]
["TECHNIK","HTI  6,4 zelená R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 6,4/3,2mm UL zelená (cívka 75m)","75m",26.44265562198693,{"$f":"F4243*(1-Elteq!$F$9)","v":26.44265562198693},"8591735044213"]
["TECHNIK","HTI  6,4 žlutá R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 6,4/3,2mm UL žlutá (cívka 75m)","75m",26.44265562198693,{"$f":"F4244*(1-Elteq!$F$9)","v":26.44265562198693},"8591735038052"]
["TECHNIK","HTI  6,4 žlutá T1",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 6,4/3,2mm žlutá pro tisk (cívka 100m)","100m",54.184248713124092,{"$f":"F4245*(1-Elteq!$F$9)","v":54.184248713124092},"8591735051242"]
["TECHNIK","HTI  6,4 žlutá T3",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 6,4/3,2mm žlutá pro tisk (cívka30m) plochá","30m",17.81399957691751,{"$f":"F4246*(1-Elteq!$F$9)","v":17.81399957691751},"8591735045845"]
["TECHNIK","HTI  6,4 žz R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 6,4/3,2mm UL žluto-zelená (cívka 75m)","75m",31.731186746384314,{"$f":"F4247*(1-Elteq!$F$9)","v":31.731186746384314},"8591735044190"]
["TECHNIK","HTI  7,0 černá R",null,"Smršťovací trubice samozhášivá, průměr 7,0/3,5mm černá (cívka 75m)","75m",29.318874303676736,{"$f":"F4248*(1-Elteq!$F$9)","v":29.318874303676736},"8591735037567"]
["TECHNIK","HTI  8,0 černá R",null,"Smršťovací trubice samozhášivá, průměr 8,0/2,0mm černá (cívka 50m)","50m",34.700186675870569,{"$f":"F4249*(1-Elteq!$F$9)","v":34.700186675870569},"8591735044244"]
["TECHNIK","HTI  9,5 bílá R",null,"Smršťovací trubice samozhášivá, průměr 9,5/4,8mm bílá (cívka 75m)","75m",32.287874233162988,{"$f":"F4250*(1-Elteq!$F$9)","v":32.287874233162988},"8591735044251"]
["TECHNIK","HTI  9,5 bílá T3",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 9,5/4,8mm bílá pro tisk (cívka30m) plochá","30m",21.154124497589542,{"$f":"F4251*(1-Elteq!$F$9)","v":21.154124497589542},"8591735045852"]
["TECHNIK","HTI  9,5 černá R",null,"Smršťovací trubice samozhášivá, průměr 9,5/4,8mm černá (cívka 75m)","75m",32.287874233162988,{"$f":"F4252*(1-Elteq!$F$9)","v":32.287874233162988},"8591735015589"]
["TECHNIK","HTI  9,5 modrá R",null,"Smršťovací trubice samozhášivá, průměr 9,5/4,8mm modrá (cívka 75m)","75m",32.287874233162988,{"$f":"F4253*(1-Elteq!$F$9)","v":32.287874233162988},"8591735044282"]
["TECHNIK","HTI  9,5 oranž R",null,"Smršťovací trubice samozhášivá, průměr 9,5/4,8mm oranžová (cívka 75m)","75m",32.287874233162988,{"$f":"F4254*(1-Elteq!$F$9)","v":32.287874233162988},"8591735052997"]
["TECHNIK","HTI  9,5 rudá R",null,"Smršťovací trubice samozhášivá, průměr 9,5/4,8mm rudá (cívka 75m)","75m",32.287874233162988,{"$f":"F4255*(1-Elteq!$F$9)","v":32.287874233162988},"8591735044305"]
["TECHNIK","HTI  9,5 šedá R",null,"Smršťovací trubice samozhášivá, průměr 9,5/4,8mm šedá (cívka 75m)","75m",32.287874233162988,{"$f":"F4256*(1-Elteq!$F$9)","v":32.287874233162988},"8591735043544"]
["TECHNIK","HTI  9,5 transp R",null,"Smršťovací trubice tenkostěnná, průměr 9,5/4,8mm transparentní (cívka 75m)","75m",32.287874233162988,{"$f":"F4257*(1-Elteq!$F$9)","v":32.287874233162988},"8591735044329"]
["TECHNIK","HTI  9,5 zelená R",null,"Smršťovací trubice samozhášivá, průměr 9,5/4,8mm zelená (cívka 75m)","75m",32.287874233162988,{"$f":"F4258*(1-Elteq!$F$9)","v":32.287874233162988},"8591735037697"]
["TECHNIK","HTI  9,5 žlutá R",null,"Smršťovací trubice samozhášivá, průměr 9,5/4,8mm žlutá (cívka 75m)","75m",32.287874233162988,{"$f":"F4259*(1-Elteq!$F$9)","v":32.287874233162988},"8591735044336"]
["TECHNIK","HTI  9,5 žlutá T3",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 9,5/4,8mm žlutá pro tisk (cívka30m) plochá","30m",21.154124497589542,{"$f":"F4260*(1-Elteq!$F$9)","v":21.154124497589542},"8591735045869"]
["TECHNIK","HTI  9,5 žz R",null,"Smršťovací trubice samozhášivá, průměr 9,5/4,8mm žluto-zelená (cívka 75m)","75m",40.916530278232408,{"$f":"F4261*(1-Elteq!$F$9)","v":40.916530278232408},"8591735044350"]
["TECHNIK","HTI 12,0 černá R",null,"Smršťovací trubice samozhášivá, průměr 12,0/6,0mm černá (cívka 50m)","50m",27.83437433893361,{"$f":"F4262*(1-Elteq!$F$9)","v":27.83437433893361},"8591735050290"]
["TECHNIK","HTI 12,7 bílá R",null,"Smršťovací trubice samozhášivá 12,7/6,4mm bílá (cívka 50m)","50m",25.9787493830047,{"$f":"F4263*(1-Elteq!$F$9)","v":25.9787493830047},"8591735035488"]
["TECHNIK","HTI 12,7 černá R",null,"Smršťovací trubice samozhášivá 12,7/6,4mm černá (cívka 50m)","50m",25.9787493830047,{"$f":"F4264*(1-Elteq!$F$9)","v":25.9787493830047},"8591735016982"]
["TECHNIK","HTI 12,7 modrá R",null,"Smršťovací trubice samozhášivá 12,7/6,4mm modrá (cívka 50m)","50m",25.9787493830047,{"$f":"F4265*(1-Elteq!$F$9)","v":25.9787493830047},"8591735044473"]
["TECHNIK","HTI 12,7 oranž R",null,"Smršťovací trubice samozhášivá 12,7/6,4mm oranžová (cívka 50m)","50m",25.9787493830047,{"$f":"F4266*(1-Elteq!$F$9)","v":25.9787493830047},"8591735054045"]
["TECHNIK","HTI 12,7 rudá R",null,"Smršťovací trubice samozhášivá 12,7/6,4mm rudá (cívka 50m)","50m",25.9787493830047,{"$f":"F4267*(1-Elteq!$F$9)","v":25.9787493830047},"8591735044459"]
["TECHNIK","HTI 12,7 šedá R",null,"Smršťovací trubice samozhášivá 12,7/6,4mm šedá (cívka 50m)","50m",25.9787493830047,{"$f":"F4268*(1-Elteq!$F$9)","v":25.9787493830047},"8591735044442"]
["TECHNIK","HTI 12,7 transp R",null,"Smršťovací trubice tenkostěnná 12,7/6,4mm transparentní (cívka 50m)","50m",25.9787493830047,{"$f":"F4269*(1-Elteq!$F$9)","v":25.9787493830047},"8591735044428"]
["TECHNIK","HTI 12,7 zelená R",null,"Smršťovací trubice samozhášivá 12,7/6,4mm zelená (cívka 50m)","50m",25.9787493830047,{"$f":"F4270*(1-Elteq!$F$9)","v":25.9787493830047},"8591735056025"]
["TECHNIK","HTI 12,7 žlutá R",null,"Smršťovací trubice samozhášivá 12,7/6,4mm žlutá (cívka 50m)","50m",25.9787493830047,{"$f":"F4271*(1-Elteq!$F$9)","v":25.9787493830047},"8591735044411"]
["TECHNIK","HTI 12,7 žz R",null,"Smršťovací trubice samozhášivá 12,7/6,4mm žluto-zelená (cívka 50m)","50m",48.246248854151588,{"$f":"F4272*(1-Elteq!$F$9)","v":48.246248854151588},"8591735043803"]
["TECHNIK","HTI 16,0 černá R",null,"Smršťovací trubice samozhášivá, průměr 16/8mm černá (cívka 50m)","50m",40.823749030435962,{"$f":"F4273*(1-Elteq!$F$9)","v":40.823749030435962},"8591735040604"]
["TECHNIK","HTI 16,0 modrá R",null,"Smršťovací trubice samozhášivá, průměr 16/8mm modrá (cívka 50m)","50m",40.823749030435962,{"$f":"F4274*(1-Elteq!$F$9)","v":40.823749030435962},"8591735040611"]
["TECHNIK","HTI 16,0 transp R",null,"Smršťovací trubice tenkostěnná, průměr 16/8mm transparentní (cívka 50m)","50m",40.823749030435962,{"$f":"F4275*(1-Elteq!$F$9)","v":40.823749030435962},"8591735040628"]
["TECHNIK","HTI 16,0 žlutá R",null,"Smršťovací trubice samozhášivá, průměr 16/8mm žlutá (cívka 50m)","50m",40.823749030435962,{"$f":"F4276*(1-Elteq!$F$9)","v":40.823749030435962},"8591735038762"]
["TECHNIK","HTI 19,0 bílá R",null,"Smršťovací trubice samozhášivá 19/9,5mm bílá (cívka 30m)","30m",30.729149270182706,{"$f":"F4277*(1-Elteq!$F$9)","v":30.729149270182706},"8591735044527"]
["TECHNIK","HTI 19,0 bílá RW",null,"Smršťovací trubice samozhášivá 19/9,5mm bílá (cívka 30m)","30m",35.44243665824213,{"$f":"F4278*(1-Elteq!$F$9)","v":35.44243665824213},""]
["TECHNIK","HTI 19,0 černá R",null,"Smršťovací trubice samozhášivá 19/9,5mm černá (cívka 30m)","30m",30.729149270182706,{"$f":"F4279*(1-Elteq!$F$9)","v":30.729149270182706},"8591735015572"]
["TECHNIK","HTI 19,0 modrá R",null,"Smršťovací trubice samozhášivá 19/9,5mm modrá (cívka 30m)","30m",30.729149270182706,{"$f":"F4280*(1-Elteq!$F$9)","v":30.729149270182706},"8591735038809"]
["TECHNIK","HTI 19,0 rudá R",null,"Smršťovací trubice samozhášivá 19/9,5mm rudá (cívka 30m)","30m",30.729149270182706,{"$f":"F4281*(1-Elteq!$F$9)","v":30.729149270182706},"8591735038816"]
["TECHNIK","HTI 19,0 šedá R",null,"Smršťovací trubice samozhášivá 19/9,5mm šedá (cívka 30m)","30m",30.729149270182706,{"$f":"F4282*(1-Elteq!$F$9)","v":30.729149270182706},"8591735044565"]
["TECHNIK","HTI 19,0 transp R",null,"Smršťovací trubice tenkostěnná 19/9,5mm transparentní (cívka 30m)","30m",30.729149270182706,{"$f":"F4283*(1-Elteq!$F$9)","v":30.729149270182706},"8591735044589"]
["TECHNIK","HTI 19,0 žlutá R",null,"Smršťovací trubice samozhášivá 19/9,5mm žlutá (cívka 30m)","30m",30.729149270182706,{"$f":"F4284*(1-Elteq!$F$9)","v":30.729149270182706},"8591735044596"]
["TECHNIK","HTI 19,0 žz R",null,"Smršťovací trubice samozhášivá 19/9,5mm žluto-zelená (cívka 30m)","30m",40.192836545420136,{"$f":"F4285*(1-Elteq!$F$9)","v":40.192836545420136},"8591735044619"]
["TECHNIK","HTI 25,4 bílá R",null,"Smršťovací trubice samozhášivá 25,4/12,7mm bílá (cívka 30m)","30m",41.751561508400414,{"$f":"F4286*(1-Elteq!$F$9)","v":41.751561508400414},"8591735044626"]
["TECHNIK","HTI 25,4 bílá RW",null,"Smršťovací trubice samozhášivá 25,4/12,7mm bílá (cívka 30m)","30m",47.875123862965808,{"$f":"F4287*(1-Elteq!$F$9)","v":47.875123862965808},""]
["TECHNIK","HTI 25,4 černá R",null,"Smršťovací trubice samozhášivá 25,4/12,7mm černá (cívka 30m)","30m",41.751561508400414,{"$f":"F4288*(1-Elteq!$F$9)","v":41.751561508400414},"8591735016999"]
["TECHNIK","HTI 25,4 modrá R",null,"Smršťovací trubice samozhášivá 25,4/12,7mm modrá (cívka 30m)","30m",41.751561508400414,{"$f":"F4289*(1-Elteq!$F$9)","v":41.751561508400414},"8591735036737"]
["TECHNIK","HTI 25,4 oranž R",null,"Smršťovací trubice samozhášivá 25,4/12,7mm oranžová (cívka 30m)","30m",41.751561508400414,{"$f":"F4290*(1-Elteq!$F$9)","v":41.751561508400414},"8591735054977"]
["TECHNIK","HTI 25,4 rudá R",null,"Smršťovací trubice samozhášivá 25,4/12,7mm rudá (cívka 30m)","30m",41.751561508400414,{"$f":"F4291*(1-Elteq!$F$9)","v":41.751561508400414},"8591735036720"]
["TECHNIK","HTI 25,4 šedá R",null,"Smršťovací trubice samozhášivá 25,4/12,7mm šedá (cívka 30m)","30m",41.751561508400414,{"$f":"F4292*(1-Elteq!$F$9)","v":41.751561508400414},"8591735042455"]
["TECHNIK","HTI 25,4 transp R",null,"Smršťovací trubice tenkostěnná 25,4/12,7mm transparentní (cívka 30m)","30m",41.751561508400414,{"$f":"F4293*(1-Elteq!$F$9)","v":41.751561508400414},"8591735042417"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"HTI 25,4 žlutá R",null,"Smršťovací trubice samozhášivá 25,4/12,7mm žlutá (cívka 30m)","30m",41.751561508400414,{"$f":"F4294*(1-Elteq!$F$9)","v":41.751561508400414},"8591735052751"]
["TECHNIK","HTI 25,4 žz R",null,"Smršťovací trubice samozhášivá 25,4/12,7mm žluto-zelená (cívka 30m)","30m",43.421623968736434,{"$f":"F4295*(1-Elteq!$F$9)","v":43.421623968736434},"8591735038847"]
["TECHNIK","HTI 30,0 černá R",null,"Smršťovací trubice samozhášivá 30/15mm černá (cívka 30m)","30m",58.229511117049114,{"$f":"F4296*(1-Elteq!$F$9)","v":58.229511117049114},"8591735049638"]
["TECHNIK","HTI 38,0 bílá R",null,"Smršťovací trubice samozhášivá 38,0/19,0mm bílá (cívka 30m)","30m",70.142623334112699,{"$f":"F4297*(1-Elteq!$F$9)","v":70.142623334112699},"8591735044718"]
["TECHNIK","HTI 38,0 černá R",null,"Smršťovací trubice samozhášivá 38,0/19,0mm černá (cívka 30m)","30m",70.142623334112699,{"$f":"F4298*(1-Elteq!$F$9)","v":70.142623334112699},"8591735037086"]
["TECHNIK","HTI 38,0 modrá R",null,"Smršťovací trubice samozhášivá 38,0/19,0mm modrá (cívka 30m)","30m",70.142623334112699,{"$f":"F4299*(1-Elteq!$F$9)","v":70.142623334112699},"8591735038823"]
["TECHNIK","HTI 38,0 oranž R",null,"Smršťovací trubice samozhášivá 38,0/19,0mm oranžová (cívka 30m)","30m",70.142623334112699,{"$f":"F4300*(1-Elteq!$F$9)","v":70.142623334112699},"8591735056513"]
["TECHNIK","HTI 38,0 rudá R",null,"Smršťovací trubice samozhášivá 38,0/19,0mm rudá (cívka 30m)","30m",70.142623334112699,{"$f":"F4301*(1-Elteq!$F$9)","v":70.142623334112699},"8591735038830"]
["TECHNIK","HTI 38,0 šedá R",null,"Smršťovací trubice samozhášivá 38,0/19,0mm šedá (cívka 30m)","30m",70.142623334112699,{"$f":"F4302*(1-Elteq!$F$9)","v":70.142623334112699},"8591735044787"]
["TECHNIK","HTI 38,0 transp R",null,"Smršťovací trubice tenkostěnná 38,0/19,0mm transparentní (cívka 30m)","30m",70.142623334112699,{"$f":"F4303*(1-Elteq!$F$9)","v":70.142623334112699},"8591735044794"]
["TECHNIK","HTI 38,0 žlutá R",null,"Smršťovací trubice samozhášivá 38,0/19,0mm žlutá (cívka 30m)","30m",70.142623334112699,{"$f":"F4304*(1-Elteq!$F$9)","v":70.142623334112699},"8591735046774"]
["TECHNIK","HTI 38,0 žz R",null,"Smršťovací trubice samozhášivá 38,0/19,0mm žluto-zelená (cívka 30m)","30m",82.389748043243486,{"$f":"F4305*(1-Elteq!$F$9)","v":82.389748043243486},"8591735044763"]
["TECHNIK","HTI 51,0 bílá R",null,"Smršťovací trubice samozhášivá 50,8/25,4mm bílá (cívka 30m)","30m",133.60499682688132,{"$f":"F4306*(1-Elteq!$F$9)","v":133.60499682688132},"8591735044824"]
["TECHNIK","HTI 51,0 černá R",null,"Smršťovací trubice samozhášivá 50,8/25,4mm černá (cívka 30m)","30m",133.60499682688132,{"$f":"F4307*(1-Elteq!$F$9)","v":133.60499682688132},"8591735044831"]
["TECHNIK","HTI 51,0 modrá R",null,"Smršťovací trubice samozhášivá 50,8/25,4mm modrá (cívka 30m)","30m",133.60499682688132,{"$f":"F4308*(1-Elteq!$F$9)","v":133.60499682688132},"8591735044893"]
["TECHNIK","HTI 51,0 oranž R",null,"Smršťovací trubice 2:1 samozhášivá, bezhalogenová, průměr 50,8/25,4mm oranžová (cívka 30m)","30m",133.60499682688132,{"$f":"F4309*(1-Elteq!$F$9)","v":133.60499682688132},"8591735052928"]
["TECHNIK","HTI 51,0 rudá R",null,"Smršťovací trubice samozhášivá 50,8/25,4mm rudá (cívka 30m)","30m",133.60499682688132,{"$f":"F4310*(1-Elteq!$F$9)","v":133.60499682688132},"8591735044886"]
["TECHNIK","HTI 51,0 šedá R",null,"Smršťovací trubice samozhášivá 50,8/25,4mm šedá (cívka 30m)","30m",133.60499682688132,{"$f":"F4311*(1-Elteq!$F$9)","v":133.60499682688132},"8591735044817"]
["TECHNIK","HTI 51,0 transp R",null,"Smršťovací trubice tenkostěnná 50,8/25,4mm transparentní (cívka 30m)","30m",133.60499682688132,{"$f":"F4312*(1-Elteq!$F$9)","v":133.60499682688132},"8591735044862"]
["TECHNIK","HTI 51,0 zelená R",null,"Smršťovací trubice samozhášivá 50,8/25,4mm zelená (cívka 30m)","30m",133.60499682688132,{"$f":"F4313*(1-Elteq!$F$9)","v":133.60499682688132},"8591735044855"]
["TECHNIK","HTI 51,0 žz R",null,"Smršťovací trubice samozhášivá 50,8/25,4mm žluto-zelená (cívka 30m)","30m",144.73874656245476,{"$f":"F4314*(1-Elteq!$F$9)","v":144.73874656245476},"8591735044848"]
["TECHNIK","HTI 76,2 bílá R",null,"Smršťovací trubice samozhášivá 76,2/38,1mm bílá (cívka 15m)","15m",94.636872752374273,{"$f":"F4315*(1-Elteq!$F$9)","v":94.636872752374273},"8591735052546"]
["TECHNIK","HTI 76,2 černá R",null,"Smršťovací trubice samozhášivá 76,2/38,1mm černá (cívka 15m)","15m",94.636872752374273,{"$f":"F4316*(1-Elteq!$F$9)","v":94.636872752374273},"8591735044961"]
["TECHNIK","HTI 76,2 modrá R",null,"Smršťovací trubice samozhášivá 76,2/38,1mm modrá (cívka 15m)","15m",94.636872752374273,{"$f":"F4317*(1-Elteq!$F$9)","v":94.636872752374273},"8591735045661"]
["TECHNIK","HTI 76,2 rudá R",null,"Smršťovací trubice samozhášivá 76,2/38,1mm rudá (cívka 15m)","15m",94.636872752374273,{"$f":"F4318*(1-Elteq!$F$9)","v":94.636872752374273},"8591735045012"]
["TECHNIK","HTI 76,2 šedá R",null,"Smršťovací trubice samozhášivá 76,2/38,1mm šedá (cívka 15m)","15m",94.636872752374273,{"$f":"F4319*(1-Elteq!$F$9)","v":94.636872752374273},"8591735044992"]
["TECHNIK","HTI 76,2 transp R",null,"Smršťovací trubice tenkostěnná 76,2/38,1mm transparentní (cívka 15m)","15m",94.636872752374273,{"$f":"F4320*(1-Elteq!$F$9)","v":94.636872752374273},"8591735017361"]
["TECHNIK","HTI 76,2 zelená R",null,"Smršťovací trubice samozhášivá 76,2/38,1mm zelená (cívka 15m)","15m",139.17187169466806,{"$f":"F4321*(1-Elteq!$F$9)","v":139.17187169466806},"8591735045036"]
["TECHNIK","HTI 76,2 žz R",null,"Smršťovací trubice samozhášivá 76,2/38,1mm žluto-zelená (cívka 15m)","15m",153.08905886413484,{"$f":"F4322*(1-Elteq!$F$9)","v":153.08905886413484},"8591735055004"]
["TECHNIK","HTI102,0 černá R",null,"Smršťovací trubice samozhášivá 102/51mm černá (cívka 15m)","15m",116.90437222352116,{"$f":"F4323*(1-Elteq!$F$9)","v":116.90437222352116},"8591735045043"]
["TECHNIK","HTI102,0 modrá R",null,"Smršťovací trubice samozhášivá 102/51mm modrá (cívka 15m)","15m",116.90437222352116,{"$f":"F4324*(1-Elteq!$F$9)","v":116.90437222352116},"8591735045067"]
["TECHNIK","HTI102,0 rudá R",null,"Smršťovací trubice samozhášivá 102/51mm rudá (cívka 15m)","15m",116.90437222352116,{"$f":"F4325*(1-Elteq!$F$9)","v":116.90437222352116},"8591735045081"]
["TECHNIK","HTI102,0 transp R",null,"Smršťovací trubice tenkostěnná 102/51mm transparentní (cívka 15m)","15m",116.90437222352116,{"$f":"F4326*(1-Elteq!$F$9)","v":116.90437222352116},"8591735043797"]
["TECHNIK","HTI180,0 černá",null,"Smršťovací trubice samozhášivá 180/90mm černá 0,85mm před smrštěním (cívka 20m)","1m",32.918786718178815,{"$f":"F4327*(1-Elteq!$F$9)","v":32.918786718178815},"8591735045128"]
["TECHNIK","CFW   9/3 A",null,"Smršťovací trubice silnostěnná s lepidlem, průměr 9,0/3,0mm černá","1,22m",5.1957498766009405,{"$f":"F4328*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735040048"]
["TECHNIK","CFW  12/4 A",null,"Smršťovací trubice silnostěnná s lepidlem, průměr 12,0/4,0mm černá","1,22m",6.0864498554468156,{"$f":"F4329*(1-Elteq!$F$9)","v":6.0864498554468156},"8591735016937"]
["TECHNIK","CFW  33/8 A",null,"Smršťovací trubice silnostěnná s lepidlem, průměr 33,0/8,0mm černá","1,22m",7.4967248219527853,{"$f":"F4330*(1-Elteq!$F$9)","v":7.4967248219527853},"8591735040062"]
["TECHNIK","CFW  45/13 A",null,"Smršťovací trubice silnostěnná s lepidlem, průměr 45,0/13,0mm černá","1,22m",10.836849742624819,{"$f":"F4331*(1-Elteq!$F$9)","v":10.836849742624819},"8591735040079"]
["TECHNIK","CFW  55/16 A",null,"Smršťovací trubice silnostěnná s lepidlem, průměr 55,0/16,0mm černá","1,22m",13.508949679162445,{"$f":"F4332*(1-Elteq!$F$9)","v":13.508949679162445},"8591735040086"]
["TECHNIK","CFW  65/19 A",null,"Smršťovací trubice silnostěnná s lepidlem, průměr 65,0/19,0mm černá","1,22m",16.181049615700072,{"$f":"F4333*(1-Elteq!$F$9)","v":16.181049615700072},"8591735048211"]
["TECHNIK","CFW  75/22 A",null,"Smršťovací trubice silnostěnná s lepidlem, průměr 75,0/22,0mm černá","1,22m",16.849074599834477,{"$f":"F4334*(1-Elteq!$F$9)","v":16.849074599834477},"8591735040093"]
["TECHNIK","CFW  85/25 A",null,"Smršťovací trubice silnostěnná s lepidlem, průměr 85,0/25,0mm černá","1,22m",21.525249488775323,{"$f":"F4335*(1-Elteq!$F$9)","v":21.525249488775323},"8591735048228"]
["TECHNIK","CFW  95/30 A",null,"Smršťovací trubice silnostěnná s lepidlem, průměr 95,0/30,0mm černá","1,22m",22.490174465858356,{"$f":"F4336*(1-Elteq!$F$9)","v":22.490174465858356},"8591735040109"]
["TECHNIK","CFW 105/30 A",null,"Smršťovací trubice silnostěnná s lepidlem, průměr 105,0/30,0mm černá","1,22m",26.461211871546219,{"$f":"F4337*(1-Elteq!$F$9)","v":26.461211871546219},"8591735048235"]
["TECHNIK","CFW 115/34 A",null,"Smršťovací trubice silnostěnná s lepidlem, průměr 115,0/34,0mm černá","1,22m",30.024011786929719,{"$f":"F4338*(1-Elteq!$F$9)","v":30.024011786929719},"8591735048242"]
["TECHNIK","CFW 140/42 A",null,"Smršťovací trubice silnostěnná s lepidlem, průměr 140,0/42,0mm černá","1,22m",38.81967407803274,{"$f":"F4339*(1-Elteq!$F$9)","v":38.81967407803274},"8591735048204"]
["TECHNIK","CFW 175/50 A",null,"Smršťovací trubice silnostěnná s lepidlem, průměr 175,0/50,0mm černá","1,22m",60.678936058875266,{"$f":"F4340*(1-Elteq!$F$9)","v":60.678936058875266},"8591735048785"]
["TECHNIK","CFW 200/60 A",null,"Smršťovací trubice silnostěnná s lepidlem, průměr 200,0/60,0mm černá","1,22m",76.080623193085202,{"$f":"F4341*(1-Elteq!$F$9)","v":76.080623193085202},"8591735048792"]
["TECHNIK","RBH  15/6",null,"Smršťovací trubice silnostěnná do 36 kV","1m",13.137824687976664,{"$f":"F4342*(1-Elteq!$F$9)","v":13.137824687976664},"8591735042950"]
["TECHNIK","RBH  25/10",null,"Smršťovací trubice silnostěnná do 36 kV","1m",15.030562143024149,{"$f":"F4343*(1-Elteq!$F$9)","v":15.030562143024149},"8591735042967"]
["TECHNIK","RBH  30/12",null,"Smršťovací trubice silnostěnná do 36 kV","1m",17.888224575154666,{"$f":"F4344*(1-Elteq!$F$9)","v":17.888224575154666},"8591735042974"]
["TECHNIK","RBH  40/16",null,"Smršťovací trubice silnostěnná do 36 kV","1m",24.345799421787262,{"$f":"F4345*(1-Elteq!$F$9)","v":24.345799421787262},"8591735042981"]
["TECHNIK","RBH  50/20",null,"Smršťovací trubice silnostěnná do 36 kV","1m",26.795224363613421,{"$f":"F4346*(1-Elteq!$F$9)","v":26.795224363613421},""]
["TECHNIK","RBH  65/25",null,"Smršťovací trubice silnostěnná do 36 kV","1m",29.05908680984669,{"$f":"F4347*(1-Elteq!$F$9)","v":29.05908680984669},""]
["TECHNIK","RBH  75/30",null,"Smršťovací trubice silnostěnná do 36 kV","1m",34.588849178514835,{"$f":"F4348*(1-Elteq!$F$9)","v":34.588849178514835},""]
["TECHNIK","RBH  85/35",null,"Smršťovací trubice silnostěnná do 36 kV","1m",39.636149058641458,{"$f":"F4349*(1-Elteq!$F$9)","v":39.636149058641458},""]
["TECHNIK","RBH 100/40",null,"Smršťovací trubice silnostěnná do 36 kV","1m",45.054573929953868,{"$f":"F4350*(1-Elteq!$F$9)","v":45.054573929953868},""]
["TECHNIK","RBH 120/50",null,"Smršťovací trubice silnostěnná do 36 kV","1m",48.988498836523149,{"$f":"F4351*(1-Elteq!$F$9)","v":48.988498836523149},""]
["TECHNIK","RBH 150/60",null,"Smršťovací trubice silnostěnná do 36 kV","1m",73.482748254784724,{"$f":"F4352*(1-Elteq!$F$9)","v":73.482748254784724},""]
["TECHNIK","RGK   9/3",null,"Smršťovací trubice silnostěnná s lepidlem 9,0/3,0mm černá (CFW, TLT)","1m",4.2679373986364864,{"$f":"F4353*(1-Elteq!$F$9)","v":4.2679373986364864},"8591735048075"]
["TECHNIK","RGK  12/4",null,"Smršťovací trubice silnostěnná s lepidlem 12,0/4,0mm černá (CFW, TLT)","1m",4.9730748818894712,{"$f":"F4354*(1-Elteq!$F$9)","v":4.9730748818894712},"8591735048082"]
["TECHNIK","RGK  19/3,2",null,"Smršťovací trubice 6:1 silnostěnná s lepidlem 19,0/3,2mm černá (CFW, TLT)","1m",7.7936248149014107,{"$f":"F4355*(1-Elteq!$F$9)","v":7.7936248149014107},"8591735048365"]
["TECHNIK","RGK  22/6",null,"Smršťovací trubice silnostěnná s lepidlem 22,0/6,0mm černá (CFW, TLT)","1m",5.5297623686681439,{"$f":"F4356*(1-Elteq!$F$9)","v":5.5297623686681439},"8591735048068"]
["TECHNIK","RGK  33/5,5",null,"Smršťovací trubice 6:1 silnostěnná s lepidlem 33,0/5,5mm černá (CFW, TLT)","1m",9.0925622840516453,{"$f":"F4357*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735048372"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"RGK  33/8",null,"Smršťovací trubice silnostěnná s lepidlem 33,0/8,0mm černá (CFW, TLT)","1m",6.1235623545653937,{"$f":"F4358*(1-Elteq!$F$9)","v":6.1235623545653937},"8591735048020"]
["TECHNIK","RGK  44/7,4",null,"Smršťovací trubice 6:1 silnostěnná s lepidlem 44,4/7,4mm černá (CFW, TLT)","1m",13.434724680925289,{"$f":"F4359*(1-Elteq!$F$9)","v":13.434724680925289},"8591735048389"]
["TECHNIK","RGK  45/13",null,"Smršťovací trubice silnostěnná s lepidlem 45,0/13,0mm černá (CFW, TLT)","1m",8.869887289340177,{"$f":"F4360*(1-Elteq!$F$9)","v":8.869887289340177},"8591735048143"]
["TECHNIK","RGK  51/8,3",null,"Smršťovací trubice 6:1 silnostěnná s lepidlem 50,8/8,3mm černá (CFW, TLT)","1m",18.630474557526231,{"$f":"F4361*(1-Elteq!$F$9)","v":18.630474557526231},"8591735040925"]
["TECHNIK","RGK  55/16",null,"Smršťovací trubice silnostěnná s lepidlem 55,0/16,0mm černá (CFW, TLT)","1m",11.059524737336288,{"$f":"F4362*(1-Elteq!$F$9)","v":11.059524737336288},"8591735027254"]
["TECHNIK","RGK  65/19",null,"Smršťovací trubice silnostěnná s lepidlem 65,0/19,0mm černá (CFW, TLT)","1m",13.249162185332398,{"$f":"F4363*(1-Elteq!$F$9)","v":13.249162185332398},"8591735027261"]
["TECHNIK","RGK  69/11,7",null,"Smršťovací trubice 6:1 silnostěnná s lepidlem 69,8/11,7mm černá (CFW, TLT)","1m",29.838449291336829,{"$f":"F4364*(1-Elteq!$F$9)","v":29.838449291336829},"8591735048396"]
["TECHNIK","RGK  75/22",null,"Smršťovací trubice silnostěnná s lepidlem 75,0/22,0mm černá (CFW, TLT)","1m",13.805849672111071,{"$f":"F4365*(1-Elteq!$F$9)","v":13.805849672111071},"8591735048105"]
["TECHNIK","RGK  85/25",null,"Smršťovací trubice silnostěnná s lepidlem 85,0/25,0mm černá (CFW, TLT)","1m",17.62843708132462,{"$f":"F4366*(1-Elteq!$F$9)","v":17.62843708132462},"8591735048150"]
["TECHNIK","RGK  89/17,1",null,"Smršťovací trubice 6:1 silnostěnná s lepidlem 88,9/17,1mm černá (CFW, TLT)","1m",37.632074106238242,{"$f":"F4367*(1-Elteq!$F$9)","v":37.632074106238242},"8591735048402"]
["TECHNIK","RGK  95/30",null,"Smršťovací trubice silnostěnná s lepidlem 95,0/30,0mm černá (CFW, TLT)","1m",18.444912061933337,{"$f":"F4368*(1-Elteq!$F$9)","v":18.444912061933337},"8591735027278"]
["TECHNIK","RGK 105/30",null,"Smršťovací trubice silnostěnná s lepidlem 105,0/30,0mm černá (CFW, TLT)","1m",21.673699485249639,{"$f":"F4369*(1-Elteq!$F$9)","v":21.673699485249639},"8591735048112"]
["TECHNIK","RGK 115/34",null,"Smršťovací trubice silnostěnná s lepidlem 115,0/34,0mm černá (CFW, TLT)","1m",24.605586915617312,{"$f":"F4370*(1-Elteq!$F$9)","v":24.605586915617312},"8591735048129"]
["TECHNIK","RGK 119/22,9",null,"Smršťovací trubice 6:1 silnostěnná s lepidlem 119,4/22,9mm černá (CFW, TLT)","1m",49.322511328590359,{"$f":"F4371*(1-Elteq!$F$9)","v":49.322511328590359},"8591735038564"]
["TECHNIK","RGK 130/36",null,"Smršťovací trubice silnostěnná s lepidlem 130,0/36,0mm černá (CFW, TLT)","1m",29.467324300151049,{"$f":"F4372*(1-Elteq!$F$9)","v":29.467324300151049},"8591735048167"]
["TECHNIK","RGK 140/34",null,"Smršťovací trubice silnostěnná s lepidlem 140,0/34,0mm černá (CFW, TLT)","1m",31.80541174462147,{"$f":"F4373*(1-Elteq!$F$9)","v":31.80541174462147},"8591735048136"]
["TECHNIK","RGK 160/50",null,"Smršťovací trubice silnostěnná s lepidlem 160,0/50,0mm černá (CFW, TLT)","1m",42.605148988127709,{"$f":"F4374*(1-Elteq!$F$9)","v":42.605148988127709},"8591735048174"]
["TECHNIK","RGK 175/50",null,"Smršťovací trubice silnostěnná s lepidlem 175,0/50,0mm černá (CFW, TLT)","1m",49.730748818894718,{"$f":"F4375*(1-Elteq!$F$9)","v":49.730748818894718},"8591735048181"]
["TECHNIK","RGK 200/60",null,"Smršťovací trubice silnostěnná s lepidlem 200,0/60,0mm černá (CFW, TLT)","1m",62.348998519211285,{"$f":"F4376*(1-Elteq!$F$9)","v":62.348998519211285},"8591735048198"]
["TECHNIK","PBF  1,6/0,8 bílá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 1,6/0,8mm (1/16\") bílá (po 10m)","1m",0.2783437433893361,{"$f":"F4377*(1-Elteq!$F$9)","v":0.2783437433893361},"8591735014681"]
["TECHNIK","PBF  1,6/0,8 černá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 1,6/0,8mm (1/16\") černá (po 10m)","1m",0.2783437433893361,{"$f":"F4378*(1-Elteq!$F$9)","v":0.2783437433893361},"8591735014698"]
["TECHNIK","PBF  1,6/0,8 fialová",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 1,6/0,8mm (1/16\") fialová (po 10m)","1m",0.2783437433893361,{"$f":"F4379*(1-Elteq!$F$9)","v":0.2783437433893361},"8591735025168"]
["TECHNIK","PBF  1,6/0,8 hnědá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 1,6/0,8mm (1/16\") hnědá (po 10m)","1m",0.2783437433893361,{"$f":"F4380*(1-Elteq!$F$9)","v":0.2783437433893361},"8591735014704"]
["TECHNIK","PBF  1,6/0,8 modrá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 1,6/0,8mm (1/16\") modrá (po 10m)","1m",0.2783437433893361,{"$f":"F4381*(1-Elteq!$F$9)","v":0.2783437433893361},"8591735014667"]
["TECHNIK","PBF  1,6/0,8 oranž",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 1,6/0,8mm (1/16\") oranžová (po 10m)","1m",0.2783437433893361,{"$f":"F4382*(1-Elteq!$F$9)","v":0.2783437433893361},"8591735032296"]
["TECHNIK","PBF  1,6/0,8 rudá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 1,6/0,8mm (1/16\") rudá (po 10m)","1m",0.2783437433893361,{"$f":"F4383*(1-Elteq!$F$9)","v":0.2783437433893361},"8591735014711"]
["TECHNIK","PBF  1,6/0,8 transp",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 1,6/0,8mm (1/16\") transparentní (po 10m)","1m",0.2783437433893361,{"$f":"F4384*(1-Elteq!$F$9)","v":0.2783437433893361},"8591735014728"]
["TECHNIK","PBF  1,6/0,8 zelená",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 1,6/0,8mm (1/16\") zelená (po 10m)","1m",0.2783437433893361,{"$f":"F4385*(1-Elteq!$F$9)","v":0.2783437433893361},"8591735014735"]
["TECHNIK","PBF  1,6/0,8 žlutá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 1,6/0,8mm (1/16\") žlutá (po 10m)","1m",0.2783437433893361,{"$f":"F4386*(1-Elteq!$F$9)","v":0.2783437433893361},"8591735014742"]
["TECHNIK","PBF  1,6/0,8 žz",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 1,6/0,8mm (1/16\") žluto-zelená (po 10m)","1m",0.31174499259605642,{"$f":"F4387*(1-Elteq!$F$9)","v":0.31174499259605642},"8591735014759"]
["TECHNIK","PBF  2,4/1,2 bílá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 2,4/1,2mm (3/32\") bílá (po 10m)","1m",0.30061124286048296,{"$f":"F4388*(1-Elteq!$F$9)","v":0.30061124286048296},"8591735014766"]
["TECHNIK","PBF  2,4/1,2 černá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 2,4/1,2mm (3/32\") černá (po 10m)","1m",0.30061124286048296,{"$f":"F4389*(1-Elteq!$F$9)","v":0.30061124286048296},"8591735014773"]
["TECHNIK","PBF  2,4/1,2 fialová",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 2,4/1,2mm (3/32\") fialová (po 10m)","1m",0.30061124286048296,{"$f":"F4390*(1-Elteq!$F$9)","v":0.30061124286048296},"8591735021436"]
["TECHNIK","PBF  2,4/1,2 hnědá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 2,4/1,2mm (3/32\") hnědá (po 10m)","1m",0.30061124286048296,{"$f":"F4391*(1-Elteq!$F$9)","v":0.30061124286048296},"8591735014780"]
["TECHNIK","PBF  2,4/1,2 modrá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 2,4/1,2mm (3/32\") modrá (po 10m)","1m",0.30061124286048296,{"$f":"F4392*(1-Elteq!$F$9)","v":0.30061124286048296},"8591735014797"]
["TECHNIK","PBF  2,4/1,2 oranž",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 2,4/1,2mm (3/32\") oranžová (po 10m)","1m",0.30061124286048296,{"$f":"F4393*(1-Elteq!$F$9)","v":0.30061124286048296},"8591735021443"]
["TECHNIK","PBF  2,4/1,2 rudá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 2,4/1,2mm (3/32\") rudá (po 10m)","1m",0.30061124286048296,{"$f":"F4394*(1-Elteq!$F$9)","v":0.30061124286048296},"8591735014803"]
["TECHNIK","PBF  2,4/1,2 transp",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 2,4/1,2mm (3/32\") transparentní (po 10m)","1m",0.30061124286048296,{"$f":"F4395*(1-Elteq!$F$9)","v":0.30061124286048296},"8591735014810"]
["TECHNIK","PBF  2,4/1,2 zelená",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 2,4/1,2mm (3/32\") zelená (po 10m)","1m",0.30061124286048296,{"$f":"F4396*(1-Elteq!$F$9)","v":0.30061124286048296},"8591735014827"]
["TECHNIK","PBF  2,4/1,2 žlutá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 2,4/1,2mm (3/32\") žlutá (po 10m)","1m",0.30061124286048296,{"$f":"F4397*(1-Elteq!$F$9)","v":0.30061124286048296},"8591735014834"]
["TECHNIK","PBF  2,4/1,2 žz",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 2,4/1,2mm (3/32\") žluto-zelená (po 10m)","1m",0.33401249206720329,{"$f":"F4398*(1-Elteq!$F$9)","v":0.33401249206720329},"8591735014841"]
["TECHNIK","PBF  3,2/1,6 bílá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 3,2/1,6mm (1/8\") bílá (po 10m)","1m",0.31916749241977205,{"$f":"F4399*(1-Elteq!$F$9)","v":0.31916749241977205},"8591735014858"]
["TECHNIK","PBF  3,2/1,6 černá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 3,2/1,6mm (1/8\") černá (po 10m)","1m",0.31916749241977205,{"$f":"F4400*(1-Elteq!$F$9)","v":0.31916749241977205},"8591735014865"]
["TECHNIK","PBF  3,2/1,6 fialová",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 3,2/1,6mm (1/8\") fialová (po 10m)","1m",0.31916749241977205,{"$f":"F4401*(1-Elteq!$F$9)","v":0.31916749241977205},"8591735021450"]
["TECHNIK","PBF  3,2/1,6 hnědá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 3,2/1,6mm (1/8\") hnědá (po 10m)","1m",0.31916749241977205,{"$f":"F4402*(1-Elteq!$F$9)","v":0.31916749241977205},"8591735014872"]
["TECHNIK","PBF  3,2/1,6 modrá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 3,2/1,6mm (1/8\") modrá (po 10m)","1m",0.31916749241977205,{"$f":"F4403*(1-Elteq!$F$9)","v":0.31916749241977205},"8591735014421"]
["TECHNIK","PBF  3,2/1,6 oranž",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 3,2/1,6mm (1/8\") oranžová (po 10m)","1m",0.31916749241977205,{"$f":"F4404*(1-Elteq!$F$9)","v":0.31916749241977205},"8591735038519"]
["TECHNIK","PBF  3,2/1,6 rudá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 3,2/1,6mm (1/8\") rudá (po 10m)","1m",0.31916749241977205,{"$f":"F4405*(1-Elteq!$F$9)","v":0.31916749241977205},"8591735014896"]
["TECHNIK","PBF  3,2/1,6 šedá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 3,2/1,6mm (1/8\") šedá (po 10m)","1m",0.31916749241977205,{"$f":"F4406*(1-Elteq!$F$9)","v":0.31916749241977205},"8591735025182"]
["TECHNIK","PBF  3,2/1,6 transp",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 3,2/1,6mm (1/8\") transparentní (po 10m)","1m",0.31916749241977205,{"$f":"F4407*(1-Elteq!$F$9)","v":0.31916749241977205},"8591735014889"]
["TECHNIK","PBF  3,2/1,6 zelená",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 3,2/1,6mm (1/8\") zelená (po 10m)","1m",0.31916749241977205,{"$f":"F4408*(1-Elteq!$F$9)","v":0.31916749241977205},"8591735014902"]
["TECHNIK","PBF  3,2/1,6 žlutá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 3,2/1,6mm (1/8\") žlutá (po 10m)","1m",0.31916749241977205,{"$f":"F4409*(1-Elteq!$F$9)","v":0.31916749241977205},"8591735014919"]
["TECHNIK","PBF  3,2/1,6 žz",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 3,2/1,6mm (1/8\") žluto-zelená (po 10m)","1m",0.37112499118578146,{"$f":"F4410*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735014926"]
["TECHNIK","PBF  4,8/2,4 bílá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 4,8/2,4mm (3/16\") bílá (po 10m)","1m",0.37112499118578146,{"$f":"F4411*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735014933"]
["TECHNIK","PBF  4,8/2,4 černá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 4,8/2,4mm (3/16\") černá (po 10m)","1m",0.37112499118578146,{"$f":"F4412*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735014384"]
["TECHNIK","PBF  4,8/2,4 fialová",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 4,8/2,4mm (3/16\") fialová (po 10m)","1m",0.37112499118578146,{"$f":"F4413*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735027896"]
["TECHNIK","PBF  4,8/2,4 hnědá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 4,8/2,4mm (3/16\") hnědá (po 10m)","1m",0.37112499118578146,{"$f":"F4414*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735014940"]
["TECHNIK","PBF  4,8/2,4 modrá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 4,8/2,4mm (3/16\") modrá (po 10m)","1m",0.37112499118578146,{"$f":"F4415*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735014636"]
["TECHNIK","PBF  4,8/2,4 oranž",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 4,8/2,4mm (3/16\") oranžová (po 10m)","1m",0.37112499118578146,{"$f":"F4416*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735019037"]
["TECHNIK","PBF  4,8/2,4 rudá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 4,8/2,4mm (3/16\") rudá (po 10m)","1m",0.37112499118578146,{"$f":"F4417*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735014445"]
["TECHNIK","PBF  4,8/2,4 šedá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 4,8/2,4mm (3/16\") šedá (po 10m)","1m",0.37112499118578146,{"$f":"F4418*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735032302"]
["TECHNIK","PBF  4,8/2,4 transp",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 4,8/2,4mm (3/16\") transparentní (po 10m)","1m",0.37112499118578146,{"$f":"F4419*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735007447"]
["TECHNIK","PBF  4,8/2,4 zelená",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 4,8/2,4mm (3/16\") zelená (po 10m)","1m",0.37112499118578146,{"$f":"F4420*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735014957"]
["TECHNIK","PBF  4,8/2,4 žlutá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 4,8/2,4mm (3/16\") žlutá (po 10m)","1m",0.37112499118578146,{"$f":"F4421*(1-Elteq!$F$9)","v":0.37112499118578146},"8591735014964"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"PBF  4,8/2,4 žz",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 4,8/2,4mm (3/16\") žluto-zelená (po 10m)","1m",0.40823749030435963,{"$f":"F4422*(1-Elteq!$F$9)","v":0.40823749030435963},"8591735014407"]
["TECHNIK","PBF  4/1 bílá",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 4,0/1,0mm barva bílá (po 10m)","1m",0.52699748748380959,{"$f":"F4423*(1-Elteq!$F$9)","v":0.52699748748380959},"8591735020125"]
["TECHNIK","PBF  4/1 černá",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 4,0/1,0mm barva černá (po 10m)","1m",0.52699748748380959,{"$f":"F4424*(1-Elteq!$F$9)","v":0.52699748748380959},"8591735014971"]
["TECHNIK","PBF  4/1 fialová",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 4,0/1,0mm barva fialová (po 10m)","1m",0.52699748748380959,{"$f":"F4425*(1-Elteq!$F$9)","v":0.52699748748380959},"8591735021252"]
["TECHNIK","PBF  4/1 hnědá",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 4,0/1,0mm barva hnědá (po 10m)","1m",0.52699748748380959,{"$f":"F4426*(1-Elteq!$F$9)","v":0.52699748748380959},"8591735025199"]
["TECHNIK","PBF  4/1 modrá",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 4,0/1,0mm barva modrá (po 10m)","1m",0.52699748748380959,{"$f":"F4427*(1-Elteq!$F$9)","v":0.52699748748380959},"8591735018955"]
["TECHNIK","PBF  4/1 oranž",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 4,0/1,0mm barva oranžová (po 10m)","1m",0.52699748748380959,{"$f":"F4428*(1-Elteq!$F$9)","v":0.52699748748380959},"8591735021399"]
["TECHNIK","PBF  4/1 rudá",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 4,0/1,0mm barva rudá (po 10m)","1m",0.52699748748380959,{"$f":"F4429*(1-Elteq!$F$9)","v":0.52699748748380959},"8591735021405"]
["TECHNIK","PBF  4/1 transp",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 4,0/1,0mm barva transparentní (po 10m)","1m",0.52699748748380959,{"$f":"F4430*(1-Elteq!$F$9)","v":0.52699748748380959},"8591735020880"]
["TECHNIK","PBF  4/1 zelená",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 4,0/1,0mm barva zelená (po 10m)","1m",0.52699748748380959,{"$f":"F4431*(1-Elteq!$F$9)","v":0.52699748748380959},"8591735021412"]
["TECHNIK","PBF  4/1 žlutá",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 4,0/1,0mm barva žlutá (po 10m)","1m",0.52699748748380959,{"$f":"F4432*(1-Elteq!$F$9)","v":0.52699748748380959},"8591735019112"]
["TECHNIK","PBF  4/1 žz",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 4,0/1,0mm barva žluto-zelená (po 10m)","1m",0.58637748607353468,{"$f":"F4433*(1-Elteq!$F$9)","v":0.58637748607353468},"8591735019099"]
["TECHNIK","PBF  6,4/3,2 bílá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 6,4/3,2mm (1/4\") bílá (po 10m)","1m",0.46761748889408461,{"$f":"F4434*(1-Elteq!$F$9)","v":0.46761748889408461},"8591735014988"]
["TECHNIK","PBF  6,4/3,2 černá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 6,4/3,2mm (1/4\") černá (po 10m)","1m",0.46761748889408461,{"$f":"F4435*(1-Elteq!$F$9)","v":0.46761748889408461},"8591735014544"]
["TECHNIK","PBF  6,4/3,2 fialová",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 6,4/3,2mm (1/4\") fialová (po 10m)","1m",0.46761748889408461,{"$f":"F4436*(1-Elteq!$F$9)","v":0.46761748889408461},"8591735021269"]
["TECHNIK","PBF  6,4/3,2 hnědá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 6,4/3,2mm (1/4\") hnědá (po 10m)","1m",0.46761748889408461,{"$f":"F4437*(1-Elteq!$F$9)","v":0.46761748889408461},"8591735014995"]
["TECHNIK","PBF  6,4/3,2 modrá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 6,4/3,2mm (1/4\") modrá (po 10m)","1m",0.46761748889408461,{"$f":"F4438*(1-Elteq!$F$9)","v":0.46761748889408461},"8591735014612"]
["TECHNIK","PBF  6,4/3,2 oranž",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 6,4/3,2mm (1/4\") oranžová (po 10m)","1m",0.46761748889408461,{"$f":"F4439*(1-Elteq!$F$9)","v":0.46761748889408461},"8591735025151"]
["TECHNIK","PBF  6,4/3,2 rudá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 6,4/3,2mm (1/4\") rudá (po 10m)","1m",0.46761748889408461,{"$f":"F4440*(1-Elteq!$F$9)","v":0.46761748889408461},"8591735014629"]
["TECHNIK","PBF  6,4/3,2 šedá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 6,4/3,2mm (1/4\") šedá (po 10m)","1m",0.46761748889408461,{"$f":"F4441*(1-Elteq!$F$9)","v":0.46761748889408461},"8591735025144"]
["TECHNIK","PBF  6,4/3,2 transp",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 6,4/3,2mm (1/4\") transparentní (po 10m)","1m",0.46761748889408461,{"$f":"F4442*(1-Elteq!$F$9)","v":0.46761748889408461},"8591735014452"]
["TECHNIK","PBF  6,4/3,2 zelená",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 6,4/3,2mm (1/4\") zelená (po 10m)","1m",0.46761748889408461,{"$f":"F4443*(1-Elteq!$F$9)","v":0.46761748889408461},"8591735015008"]
["TECHNIK","PBF  6,4/3,2 žlutá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 6,4/3,2mm (1/4\") žlutá (po 10m)","1m",0.46761748889408461,{"$f":"F4444*(1-Elteq!$F$9)","v":0.46761748889408461},"8591735015015"]
["TECHNIK","PBF  6,4/3,2 žz",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 6,4/3,2mm (1/4\") žluto-zelená (po 10m)","1m",0.52699748748380959,{"$f":"F4445*(1-Elteq!$F$9)","v":0.52699748748380959},"8591735014377"]
["TECHNIK","PBF  8/2 bílá",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 8,0/2,0mm barva bílá (po 10m)","1m",0.74224998237156292,{"$f":"F4446*(1-Elteq!$F$9)","v":0.74224998237156292},"8591735015022"]
["TECHNIK","PBF  8/2 černá",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 8,0/2,0mm barva černá (po 10m)","1m",0.74224998237156292,{"$f":"F4447*(1-Elteq!$F$9)","v":0.74224998237156292},"8591735015039"]
["TECHNIK","PBF  8/2 fialová",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 8,0/2,0mm barva fialová (po 10m)","1m",0.74224998237156292,{"$f":"F4448*(1-Elteq!$F$9)","v":0.74224998237156292},"8591735021474"]
["TECHNIK","PBF  8/2 hnědá",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 8,0/2,0mm barva hnědá (po 10m)","1m",0.74224998237156292,{"$f":"F4449*(1-Elteq!$F$9)","v":0.74224998237156292},"8591735021467"]
["TECHNIK","PBF  8/2 modrá",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 8,0/2,0mm barva modrá (po 10m)","1m",0.74224998237156292,{"$f":"F4450*(1-Elteq!$F$9)","v":0.74224998237156292},"8591735015046"]
["TECHNIK","PBF  8/2 oranž",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 8,0/2,0mm barva oranžová (po 10m)","1m",0.74224998237156292,{"$f":"F4451*(1-Elteq!$F$9)","v":0.74224998237156292},"8591735032326"]
["TECHNIK","PBF  8/2 rudá",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 8,0/2,0mm barva rudá (po 10m)","1m",0.74224998237156292,{"$f":"F4452*(1-Elteq!$F$9)","v":0.74224998237156292},"8591735015053"]
["TECHNIK","PBF  8/2 šedá",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 8,0/2,0mm barva šedá (po 10m)","1m",0.74224998237156292,{"$f":"F4453*(1-Elteq!$F$9)","v":0.74224998237156292},"8591735032333"]
["TECHNIK","PBF  8/2 transp",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 8,0/2,0mm barva transparentní (po 10m)","1m",0.74224998237156292,{"$f":"F4454*(1-Elteq!$F$9)","v":0.74224998237156292},"8591735015060"]
["TECHNIK","PBF  8/2 zelená",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 8,0/2,0mm barva zelená (po 10m)","1m",0.74224998237156292,{"$f":"F4455*(1-Elteq!$F$9)","v":0.74224998237156292},"8591735015077"]
["TECHNIK","PBF  8/2 žlutá",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 8,0/2,0mm barva žlutá (po 10m)","1m",0.74224998237156292,{"$f":"F4456*(1-Elteq!$F$9)","v":0.74224998237156292},"8591735016494"]
["TECHNIK","PBF  8/2 žz",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 8,0/2,0mm barva žluto-zelená (po 10m)","1m",0.77936248149014109,{"$f":"F4457*(1-Elteq!$F$9)","v":0.77936248149014109},"8591735015084"]
["TECHNIK","PBF  9,5/4,8 bílá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 9,5/4,8mm (3/8\") bílá (po 10m)","1m",0.54926498695495662,{"$f":"F4458*(1-Elteq!$F$9)","v":0.54926498695495662},"8591735015091"]
["TECHNIK","PBF  9,5/4,8 černá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 9,5/4,8mm (3/8\") černá (po 10m)","1m",0.54926498695495662,{"$f":"F4459*(1-Elteq!$F$9)","v":0.54926498695495662},"8591735015107"]
["TECHNIK","PBF  9,5/4,8 fialová",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 9,5/4,8mm (3/8\") fialová (po 10m)","1m",0.54926498695495662,{"$f":"F4460*(1-Elteq!$F$9)","v":0.54926498695495662},"8591735021481"]
["TECHNIK","PBF  9,5/4,8 hnědá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 9,5/4,8mm (3/8\") hnědá (po 10m)","1m",0.54926498695495662,{"$f":"F4461*(1-Elteq!$F$9)","v":0.54926498695495662},"8591735019624"]
["TECHNIK","PBF  9,5/4,8 modrá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 9,5/4,8mm (3/8\") modrá (po 10m)","1m",0.54926498695495662,{"$f":"F4462*(1-Elteq!$F$9)","v":0.54926498695495662},"8591735015114"]
["TECHNIK","PBF  9,5/4,8 oranž",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 9,5/4,8mm (3/8\") oranžová (po 10m)","1m",0.54926498695495662,{"$f":"F4463*(1-Elteq!$F$9)","v":0.54926498695495662},"8591735025243"]
["TECHNIK","PBF  9,5/4,8 rudá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 9,5/4,8mm (3/8\") rudá (po 10m)","1m",0.54926498695495662,{"$f":"F4464*(1-Elteq!$F$9)","v":0.54926498695495662},"8591735015121"]
["TECHNIK","PBF  9,5/4,8 šedá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 9,5/4,8mm (3/8\") šedá (po 10m)","1m",0.54926498695495662,{"$f":"F4465*(1-Elteq!$F$9)","v":0.54926498695495662},"8591735032340"]
["TECHNIK","PBF  9,5/4,8 transp",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 9,5/4,8mm (3/8\") transparentní (po 10m)","1m",0.54926498695495662,{"$f":"F4466*(1-Elteq!$F$9)","v":0.54926498695495662},"8591735015138"]
["TECHNIK","PBF  9,5/4,8 zelená",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 9,5/4,8mm (3/8\") zelená (po 10m)","1m",0.54926498695495662,{"$f":"F4467*(1-Elteq!$F$9)","v":0.54926498695495662},"8591735015145"]
["TECHNIK","PBF  9,5/4,8 žlutá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 9,5/4,8mm (3/8\") žlutá (po 10m)","1m",0.54926498695495662,{"$f":"F4468*(1-Elteq!$F$9)","v":0.54926498695495662},"8591735015152"]
["TECHNIK","PBF  9,5/4,8 žz",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 9,5/4,8mm (3/8\") žluto-zelená (po 10m)","1m",0.62348998519211285,{"$f":"F4469*(1-Elteq!$F$9)","v":0.62348998519211285},"8591735015169"]
["TECHNIK","PBF 12,7/6,4 bílá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 12,7/6,4mm (1/2\") bílá (po 10m)","1m",0.93523497778816922,{"$f":"F4470*(1-Elteq!$F$9)","v":0.93523497778816922},"8591735015176"]
["TECHNIK","PBF 12,7/6,4 černá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 12,7/6,4mm (1/2\") černá (po 10m)","1m",0.93523497778816922,{"$f":"F4471*(1-Elteq!$F$9)","v":0.93523497778816922},"8591735014650"]
["TECHNIK","PBF 12,7/6,4 fialová",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 12,7/6,4mm (1/2\") fialová (po 10m)","1m",0.93523497778816922,{"$f":"F4472*(1-Elteq!$F$9)","v":0.93523497778816922},"8591735021511"]
["TECHNIK","PBF 12,7/6,4 hnědá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 12,7/6,4mm (1/2\") hnědá (po 10m)","1m",0.93523497778816922,{"$f":"F4473*(1-Elteq!$F$9)","v":0.93523497778816922},"8591735015183"]
["TECHNIK","PBF 12,7/6,4 modrá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 12,7/6,4mm (1/2\") modrá (po 10m)","1m",0.93523497778816922,{"$f":"F4474*(1-Elteq!$F$9)","v":0.93523497778816922},"8591735014674"]
["TECHNIK","PBF 12,7/6,4 oranž",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 12,7/6,4mm (1/2\") oranžová (po 10m)","1m",0.93523497778816922,{"$f":"F4475*(1-Elteq!$F$9)","v":0.93523497778816922},"8591735021504"]
["TECHNIK","PBF 12,7/6,4 rudá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 12,7/6,4mm (1/2\") rudá (po 10m)","1m",0.93523497778816922,{"$f":"F4476*(1-Elteq!$F$9)","v":0.93523497778816922},"8591735015190"]
["TECHNIK","PBF 12,7/6,4 šedá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 12,7/6,4mm (1/2\") šedá (po 10m)","1m",0.93523497778816922,{"$f":"F4477*(1-Elteq!$F$9)","v":0.93523497778816922},"8591735032357"]
["TECHNIK","PBF 12,7/6,4 transp",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 12,7/6,4mm (1/2\") transparentní (po 10m)","1m",0.93523497778816922,{"$f":"F4478*(1-Elteq!$F$9)","v":0.93523497778816922},"8591735015206"]
["TECHNIK","PBF 12,7/6,4 zelená",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 12,7/6,4mm (1/2\") zelená (po 10m)","1m",0.93523497778816922,{"$f":"F4479*(1-Elteq!$F$9)","v":0.93523497778816922},"8591735015213"]
["TECHNIK","PBF 12,7/6,4 žlutá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 12,7/6,4mm (1/2\") žlutá (po 10m)","1m",0.93523497778816922,{"$f":"F4480*(1-Elteq!$F$9)","v":0.93523497778816922},"8591735015220"]
["TECHNIK","PBF 12,7/6,4 žz",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 12,7/6,4mm (1/2\") žluto-zelená (po 10m)","1m",1.0911074740861975,{"$f":"F4481*(1-Elteq!$F$9)","v":1.0911074740861975},"8591735014360"]
["TECHNIK","PBF 19/9,5 bílá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 19/9,5mm (3/4\") bílá","1m",1.3249162185332399,{"$f":"F4482*(1-Elteq!$F$9)","v":1.3249162185332399},"8591735015237"]
["TECHNIK","PBF 19/9,5 černá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 19/9,5mm (3/4\") černá (po 10m)","1m",1.3249162185332399,{"$f":"F4483*(1-Elteq!$F$9)","v":1.3249162185332399},"8591735014353"]
["TECHNIK","PBF 19/9,5 fialová",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 19/9,5mm (3/4\") fialová","1m",1.3249162185332399,{"$f":"F4484*(1-Elteq!$F$9)","v":1.3249162185332399},"8591735025205"]
["TECHNIK","PBF 19/9,5 hnědá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 19/9,5mm (3/4\") hnědá","1m",1.3249162185332399,{"$f":"F4485*(1-Elteq!$F$9)","v":1.3249162185332399},"8591735015244"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"PBF 19/9,5 modrá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 19/9,5mm (3/4\") modrá","1m",1.3249162185332399,{"$f":"F4486*(1-Elteq!$F$9)","v":1.3249162185332399},"8591735014520"]
["TECHNIK","PBF 19/9,5 oranž",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 19/9,5mm (3/4\") oranžová","1m",1.3249162185332399,{"$f":"F4487*(1-Elteq!$F$9)","v":1.3249162185332399},"8591735025212"]
["TECHNIK","PBF 19/9,5 rudá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 19/9,5mm (3/4\") rudá","1m",1.3249162185332399,{"$f":"F4488*(1-Elteq!$F$9)","v":1.3249162185332399},"8591735015251"]
["TECHNIK","PBF 19/9,5 šedá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 19/9,5mm (3/4\") šedá","1m",1.3249162185332399,{"$f":"F4489*(1-Elteq!$F$9)","v":1.3249162185332399},"8591735032364"]
["TECHNIK","PBF 19/9,5 transp",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 19/9,5mm (3/4\") transparentní","1m",1.3249162185332399,{"$f":"F4490*(1-Elteq!$F$9)","v":1.3249162185332399},"8591735015268"]
["TECHNIK","PBF 19/9,5 zelená",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 19/9,5mm (3/4\") zelená","1m",1.3249162185332399,{"$f":"F4491*(1-Elteq!$F$9)","v":1.3249162185332399},"8591735015275"]
["TECHNIK","PBF 19/9,5 žlutá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 19/9,5mm (3/4\") žlutá","1m",1.3249162185332399,{"$f":"F4492*(1-Elteq!$F$9)","v":1.3249162185332399},"8591735015282"]
["TECHNIK","PBF 19/9,5 žz",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 19/9,5mm (3/4\") žluto-zelená","1m",1.5587249629802822,{"$f":"F4493*(1-Elteq!$F$9)","v":1.5587249629802822},"8591735014537"]
["TECHNIK","PBF 25,4/12,7bílá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 25,4/12,7mm (1\") bílá","1m",1.7925337074273244,{"$f":"F4494*(1-Elteq!$F$9)","v":1.7925337074273244},"8591735015299"]
["TECHNIK","PBF 25,4/12,7černá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 25,4/12,7mm (1\") černá","1m",1.7925337074273244,{"$f":"F4495*(1-Elteq!$F$9)","v":1.7925337074273244},"8591735014186"]
["TECHNIK","PBF 25,4/12,7fialová",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 25,4/12,7mm (1\") fialová","1m",1.7925337074273244,{"$f":"F4496*(1-Elteq!$F$9)","v":1.7925337074273244},"8591735025229"]
["TECHNIK","PBF 25,4/12,7hnědá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 25,4/12,7mm (1\") hnědá","1m",1.7925337074273244,{"$f":"F4497*(1-Elteq!$F$9)","v":1.7925337074273244},"8591735015305"]
["TECHNIK","PBF 25,4/12,7modrá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 25,4/12,7mm (1\") modrá","1m",1.7925337074273244,{"$f":"F4498*(1-Elteq!$F$9)","v":1.7925337074273244},"8591735014599"]
["TECHNIK","PBF 25,4/12,7oranž",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 25,4/12,7mm (1\") oranžová","1m",1.7925337074273244,{"$f":"F4499*(1-Elteq!$F$9)","v":1.7925337074273244},"8591735015312"]
["TECHNIK","PBF 25,4/12,7rudá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 25,4/12,7mm (1\") rudá","1m",1.7925337074273244,{"$f":"F4500*(1-Elteq!$F$9)","v":1.7925337074273244},"8591735015329"]
["TECHNIK","PBF 25,4/12,7šedá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 25,4/12,7mm (1\") šedá","1m",1.7925337074273244,{"$f":"F4501*(1-Elteq!$F$9)","v":1.7925337074273244},"8591735032371"]
["TECHNIK","PBF 25,4/12,7transp",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 25,4/12,7mm (1\") transparentní","1m",1.7925337074273244,{"$f":"F4502*(1-Elteq!$F$9)","v":1.7925337074273244},"8591735015336"]
["TECHNIK","PBF 25,4/12,7zelená",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 25,4/12,7mm (1\") zelená","1m",1.7925337074273244,{"$f":"F4503*(1-Elteq!$F$9)","v":1.7925337074273244},"8591735015343"]
["TECHNIK","PBF 25,4/12,7žlutá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 25,4/12,7mm (1\") žlutá","1m",1.7925337074273244,{"$f":"F4504*(1-Elteq!$F$9)","v":1.7925337074273244},"8591735015350"]
["TECHNIK","PBF 25,4/12,7žz",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 25,4/12,7mm (1\") žluto-zelená","1m",1.8704699555763384,{"$f":"F4505*(1-Elteq!$F$9)","v":1.8704699555763384},"8591735014308"]
["TECHNIK","PBF 31,8/15,9 černá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 31,8/15,9mm (1 1/4\") černá","1m",2.5347836897988874,{"$f":"F4506*(1-Elteq!$F$9)","v":2.5347836897988874},"8591735054069"]
["TECHNIK","PBF 31,8/15,9 modrá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 31,8/15,9mm (1 1/4\") modrá","1m",2.5347836897988874,{"$f":"F4507*(1-Elteq!$F$9)","v":2.5347836897988874},"8591735054076"]
["TECHNIK","PBF 31,8/15,9 rudá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 31,8/15,9mm (1 1/4\") rudá","1m",2.5347836897988874,{"$f":"F4508*(1-Elteq!$F$9)","v":2.5347836897988874},"8591735054083"]
["TECHNIK","PBF 31,8/15,9 žlutá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 31,8/15,9mm (1 1/4\") žlutá","1m",2.5347836897988874,{"$f":"F4509*(1-Elteq!$F$9)","v":2.5347836897988874},"8591735054090"]
["TECHNIK","PBF 31,8/15,9 žz",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 31,8/15,9mm (1 1/4\") žluto-zelená","1m",2.8057049333645074,{"$f":"F4510*(1-Elteq!$F$9)","v":2.8057049333645074},"8591735054106"]
["TECHNIK","PBF 38/19 bílá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 38/19mm (1 1/2\") bílá","1m",2.8910636813372377,{"$f":"F4511*(1-Elteq!$F$9)","v":2.8910636813372377},"8591735015367"]
["TECHNIK","PBF 38/19 černá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 38/19mm (1 1/2\") černá","1m",2.8910636813372377,{"$f":"F4512*(1-Elteq!$F$9)","v":2.8910636813372377},"8591735014490"]
["TECHNIK","PBF 38/19 fialová",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 38/19mm (1 1/2\") fialová","1m",2.8910636813372377,{"$f":"F4513*(1-Elteq!$F$9)","v":2.8910636813372377},"8591735025236"]
["TECHNIK","PBF 38/19 hnědá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 38/19mm (1 1/2\") hnědá","1m",2.8910636813372377,{"$f":"F4514*(1-Elteq!$F$9)","v":2.8910636813372377},"8591735016500"]
["TECHNIK","PBF 38/19 modrá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 38/19mm (1 1/2\") modrá","1m",2.8910636813372377,{"$f":"F4515*(1-Elteq!$F$9)","v":2.8910636813372377},"8591735015374"]
["TECHNIK","PBF 38/19 oranž",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 38/19mm (1 1/2\") oranžová","1m",2.8910636813372377,{"$f":"F4516*(1-Elteq!$F$9)","v":2.8910636813372377},"8591735015381"]
["TECHNIK","PBF 38/19 rudá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 38/19mm (1 1/2\") rudá","1m",2.8910636813372377,{"$f":"F4517*(1-Elteq!$F$9)","v":2.8910636813372377},"8591735015398"]
["TECHNIK","PBF 38/19 šedá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 38/19mm (1 1/2\") šedá","1m",2.8910636813372377,{"$f":"F4518*(1-Elteq!$F$9)","v":2.8910636813372377},"8591735032388"]
["TECHNIK","PBF 38/19 transp",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 38/19mm (1 1/2\") transparentní","1m",2.8910636813372377,{"$f":"F4519*(1-Elteq!$F$9)","v":2.8910636813372377},"8591735015404"]
["TECHNIK","PBF 38/19 zelená",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 38/19mm (1 1/2\") zelené","1m",2.8910636813372377,{"$f":"F4520*(1-Elteq!$F$9)","v":2.8910636813372377},"8591735016517"]
["TECHNIK","PBF 38/19 žlutá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 38/19mm (1 1/2\") žlutá","1m",2.8910636813372377,{"$f":"F4521*(1-Elteq!$F$9)","v":2.8910636813372377},"8591735015411"]
["TECHNIK","PBF 38/19 žz",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 38/19mm (1 1/2\") žluto-zelená","1m",3.1582736749909999,{"$f":"F4522*(1-Elteq!$F$9)","v":3.1582736749909999},"8591735015428"]
["TECHNIK","PBF 51/25,4 bílá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 51/25,4mm (2\") bílá","1m",5.8637748607353473,{"$f":"F4523*(1-Elteq!$F$9)","v":5.8637748607353473},"8591735024628"]
["TECHNIK","PBF 51/25,4 černá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 51/25,4mm (2\") černá","1m",5.8637748607353473,{"$f":"F4524*(1-Elteq!$F$9)","v":5.8637748607353473},"8591735015435"]
["TECHNIK","PBF 51/25,4 modrá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 51/25,4mm (2\") modrá","1m",5.8637748607353473,{"$f":"F4525*(1-Elteq!$F$9)","v":5.8637748607353473},"8591735015442"]
["TECHNIK","PBF 51/25,4 oranž",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 51/25,4mm (2\") oranžová","1m",5.8637748607353473,{"$f":"F4526*(1-Elteq!$F$9)","v":5.8637748607353473},"8591735047740"]
["TECHNIK","PBF 51/25,4 rudá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 51/25,4mm (2\") rudá","1m",5.8637748607353473,{"$f":"F4527*(1-Elteq!$F$9)","v":5.8637748607353473},"8591735015459"]
["TECHNIK","PBF 51/25,4 šedá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 51/25,4mm (2\") šedá","1m",5.8637748607353473,{"$f":"F4528*(1-Elteq!$F$9)","v":5.8637748607353473},"8591735032395"]
["TECHNIK","PBF 51/25,4 transp",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 51/25,4mm (2\") transparentní","1m",5.8637748607353473,{"$f":"F4529*(1-Elteq!$F$9)","v":5.8637748607353473},"8591735015466"]
["TECHNIK","PBF 51/25,4 zelená",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 51/25,4mm (2\") zelená","1m",5.8637748607353473,{"$f":"F4530*(1-Elteq!$F$9)","v":5.8637748607353473},"8591735041410"]
["TECHNIK","PBF 51/25,4 žlutá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 51/25,4mm (2\") žlutá","1m",5.8637748607353473,{"$f":"F4531*(1-Elteq!$F$9)","v":5.8637748607353473},"8591735015473"]
["TECHNIK","PBF 51/25,4 žz",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 51/25,4mm (2\") žluto-zelená","1m",6.6802498413440663,{"$f":"F4532*(1-Elteq!$F$9)","v":6.6802498413440663},"8591735032401"]
["TECHNIK","PBF 76/38 bílá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 76/38mm (3\") bílá","1m",7.6822873175456765,{"$f":"F4533*(1-Elteq!$F$9)","v":7.6822873175456765},"8591735015480"]
["TECHNIK","PBF 76/38 černá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 76/38mm (3\") černá","1m",7.6822873175456765,{"$f":"F4534*(1-Elteq!$F$9)","v":7.6822873175456765},"8591735015497"]
["TECHNIK","PBF 76/38 modrá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 76/38mm (3\") modrá","1m",7.6822873175456765,{"$f":"F4535*(1-Elteq!$F$9)","v":7.6822873175456765},"8591735015503"]
["TECHNIK","PBF 76/38 rudá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 76/38mm (3\") rudá","1m",7.6822873175456765,{"$f":"F4536*(1-Elteq!$F$9)","v":7.6822873175456765},"8591735032418"]
["TECHNIK","PBF 76/38 transp",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 76/38mm (3\") transparentní","1m",7.6822873175456765,{"$f":"F4537*(1-Elteq!$F$9)","v":7.6822873175456765},"8591735016524"]
["TECHNIK","PBF 76/38 žlutá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 76/38mm (3\") žlutá","1m",7.6822873175456765,{"$f":"F4538*(1-Elteq!$F$9)","v":7.6822873175456765},"8591735032425"]
["TECHNIK","PBF 76/38 žz",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 76/38mm (3\") žluto-zelená","1m",8.1647498060871921,{"$f":"F4539*(1-Elteq!$F$9)","v":8.1647498060871921},"8591735032432"]
["TECHNIK","PBF102/51 černá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 102/51mm (4\") černá","1m",9.649249770830318,{"$f":"F4540*(1-Elteq!$F$9)","v":9.649249770830318},"8591735015510"]
["TECHNIK","PBF102/51 modrá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 102/51mm (4\") modrá","1m",9.649249770830318,{"$f":"F4541*(1-Elteq!$F$9)","v":9.649249770830318},"8591735038502"]
["TECHNIK","PBF102/51 rudá",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 102/51mm (4\") rudá","1m",9.649249770830318,{"$f":"F4542*(1-Elteq!$F$9)","v":9.649249770830318},"8591735046224"]
["TECHNIK","PBF102/51 transp",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 102/51mm (4\") transparentní","1m",9.649249770830318,{"$f":"F4543*(1-Elteq!$F$9)","v":9.649249770830318},"8591735032449"]
["TECHNIK","PBF  1,6/0,8 černá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 1,6/0,8mm (1/16\") černá (cívka 100m)","100m",27.83437433893361,{"$f":"F4544*(1-Elteq!$F$9)","v":27.83437433893361},"8591735045517"]
["TECHNIK","PBF  2,4/1,2 bílá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 2,4/1,2mm (3/32\") bílá (cívka 150m)","150m",45.091686429072446,{"$f":"F4545*(1-Elteq!$F$9)","v":45.091686429072446},"8591735037321"]
["TECHNIK","PBF  2,4/1,2 bílá T",null,"Smršťovací trubice 2:1 bezhalogenová, rozměr 2,4/1,2mm (3/32\") bílá vhodná k potisku (cívka 400m)","400m",120.24449714419319,{"$f":"F4546*(1-Elteq!$F$9)","v":120.24449714419319},"8591735046422"]
["TECHNIK","PBF  2,4/1,2 černá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 2,4/1,2mm (3/32\") černá (cívka 250m)","250m",75.152810715120751,{"$f":"F4547*(1-Elteq!$F$9)","v":75.152810715120751},"8591735024796"]
["TECHNIK","PBF  2,4/1,2 modrá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 2,4/1,2mm (3/32\") modrá (cívka 150m)","150m",45.091686429072446,{"$f":"F4548*(1-Elteq!$F$9)","v":45.091686429072446},"8591735045173"]
["TECHNIK","PBF  2,4/1,2 žlutá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 2,4/1,2mm (3/32\") žlutá (cívka 150m)","150m",45.091686429072446,{"$f":"F4549*(1-Elteq!$F$9)","v":45.091686429072446},"8591735046255"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"PBF  3,2/1,6 bílá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 3,2/1,6mm (1/8\") bílá (cívka 150m)","150m",47.875123862965808,{"$f":"F4550*(1-Elteq!$F$9)","v":47.875123862965808},"8591735037437"]
["TECHNIK","PBF  3,2/1,6 bílá T",null,"Smršťovací trubice 2:1 bezhalogenová, rozměr 3,2/1,6mm (1/8\") bílá vhodná k potisku (cívka 400m)","400m",127.66699696790882,{"$f":"F4551*(1-Elteq!$F$9)","v":127.66699696790882},"8591735046415"]
["TECHNIK","PBF  3,2/1,6 černá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 3,2/1,6mm (1/8\") černá (cívka 100m)","100m",31.916749241977204,{"$f":"F4552*(1-Elteq!$F$9)","v":31.916749241977204},"8591735045180"]
["TECHNIK","PBF  3,2/1,6 oranž R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 3,2/1,6mm (1/8\") oranžová (cívka 150m)","150m",47.875123862965808,{"$f":"F4553*(1-Elteq!$F$9)","v":47.875123862965808},"8591735045197"]
["TECHNIK","PBF  3,2/1,6 zelen R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 3,2/1,6mm (1/8\") zelená (cívka 100m)","100m",31.916749241977204,{"$f":"F4554*(1-Elteq!$F$9)","v":31.916749241977204},"8591735045203"]
["TECHNIK","PBF  3,2/1,6 žlutá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 3,2/1,6mm (1/8\") žlutá (cívka 150m)","150m",47.875123862965808,{"$f":"F4555*(1-Elteq!$F$9)","v":47.875123862965808},"8591735046262"]
["TECHNIK","PBF  4,8/2,4 bílá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 4,8/2,4mm (3/16\") bílá (cívka 100m)","100m",37.112499118578143,{"$f":"F4556*(1-Elteq!$F$9)","v":37.112499118578143},"8591735045968"]
["TECHNIK","PBF  4,8/2,4 bílá T",null,"Smršťovací trubice 2:1 bezhalogenová, rozměr 4,8/2,4mm (3/16\") bílá vhodná k potisku (cívka 300m)","300m",111.33749735573444,{"$f":"F4557*(1-Elteq!$F$9)","v":111.33749735573444},"8591735046569"]
["TECHNIK","PBF  4,8/2,4 černá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 4,8/2,4mm (3/16\") černá (cívka 100m)","100m",37.112499118578143,{"$f":"F4558*(1-Elteq!$F$9)","v":37.112499118578143},"8591735041885"]
["TECHNIK","PBF  4,8/2,4 oranž R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 4,8/2,4mm (3/16\") oranžová (cívka 100m)","100m",37.112499118578143,{"$f":"F4559*(1-Elteq!$F$9)","v":37.112499118578143},"8591735046316"]
["TECHNIK","PBF  4,8/2,4 žlutá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 4,8/2,4mm (3/16\") žlutá (cívka 75m)","75m",27.83437433893361,{"$f":"F4560*(1-Elteq!$F$9)","v":27.83437433893361},"8591735046279"]
["TECHNIK","PBF  4/1 bílá R",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 4,0/1,0mm barva bílá (cívka 100m)","100m",52.699748748380969,{"$f":"F4561*(1-Elteq!$F$9)","v":52.699748748380969},"8591735054137"]
["TECHNIK","PBF  6,4/3,2 bílá T",null,"Smršťovací trubice 2:1 bezhalogenová, rozměr 6,4/3,2mm (1/4\") bílá vhodná k potisku (cívka 300m)","300m",140.2852466682254,{"$f":"F4562*(1-Elteq!$F$9)","v":140.2852466682254},"8591735046576"]
["TECHNIK","PBF  6,4/3,2 černá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 6,4/3,2mm (1/4\") černá (cívka 100m)","100m",46.761748889408466,{"$f":"F4563*(1-Elteq!$F$9)","v":46.761748889408466},"8591735024758"]
["TECHNIK","PBF  6,4/3,2 žlutá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 6,4/3,2mm (1/4\") žlutá (cívka 100m)","100m",46.761748889408466,{"$f":"F4564*(1-Elteq!$F$9)","v":46.761748889408466},"8591735046293"]
["TECHNIK","PBF  8/2 bílá R",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 8,0/2,0mm barva bílá (cívka 100m)","100m",74.224998237156285,{"$f":"F4565*(1-Elteq!$F$9)","v":74.224998237156285},"8591735045210"]
["TECHNIK","PBF  8/2 černá R",null,"Smršťovací trubice 4:1 tenkostěnná, rozměr před/po smrštění 8,0/2,0mm barva černá (cívka 100m)","100m",74.224998237156285,{"$f":"F4566*(1-Elteq!$F$9)","v":74.224998237156285},"8591735045227"]
["TECHNIK","PBF  9,5/4,8 černá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 9,5/4,8mm (3/8\") černá (cívka 100m)","100m",54.926498695495653,{"$f":"F4567*(1-Elteq!$F$9)","v":54.926498695495653},"8591735024765"]
["TECHNIK","PBF  9,5/4,8 oranž R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 9,5/4,8mm (3/8\") oranžová (cívka 100m)","100m",54.926498695495653,{"$f":"F4568*(1-Elteq!$F$9)","v":54.926498695495653},"8591735048549"]
["TECHNIK","PBF 12,7/6,4 černá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 12,7/6,4mm (1/2\") černá (cívka 100m)","100m",93.523497778816932,{"$f":"F4569*(1-Elteq!$F$9)","v":93.523497778816932},"8591735024772"]
["TECHNIK","PBF 12,7/6,4 oranž R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 12,7/6,4mm (1/2\") oranžová (cívka 100m)","100m",93.523497778816932,{"$f":"F4570*(1-Elteq!$F$9)","v":93.523497778816932},"8591735038540"]
["TECHNIK","PBF 12,7/6,4 šedá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 12,7/6,4mm (1/2\") šedá (cívka 100m)","100m",93.523497778816932,{"$f":"F4571*(1-Elteq!$F$9)","v":93.523497778816932},""]
["TECHNIK","PBF 19/9,5 bílá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 19/9,5mm (3/4\") bílá (cívka 100m)","100m",132.49162185332398,{"$f":"F4572*(1-Elteq!$F$9)","v":132.49162185332398},"8591735055660"]
["TECHNIK","PBF 19/9,5 černá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 19/9,5mm (3/4\") černá (cívka 100m)","100m",132.49162185332398,{"$f":"F4573*(1-Elteq!$F$9)","v":132.49162185332398},"8591735024789"]
["TECHNIK","PBF 19/9,5 modrá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 19/9,5mm (3/4\") modrá (cívka 100m)","100m",132.49162185332398,{"$f":"F4574*(1-Elteq!$F$9)","v":132.49162185332398},"8591735038045"]
["TECHNIK","PBF 19/9,5 rudá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 19/9,5mm (3/4\") rudá (cívka 100m)","100m",132.49162185332398,{"$f":"F4575*(1-Elteq!$F$9)","v":132.49162185332398},"8591735036942"]
["TECHNIK","PBF 19/9,5 transp R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 19/9,5mm (3/4) transparentní (cívka100m)","100m",132.49162185332398,{"$f":"F4576*(1-Elteq!$F$9)","v":132.49162185332398},"8591735049393"]
["TECHNIK","PBF 19/9,5 zelená R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 19/9,5mm (3/4\") zelená (cívka 100m)","100m",132.49162185332398,{"$f":"F4577*(1-Elteq!$F$9)","v":132.49162185332398},"8591735036461"]
["TECHNIK","PBF 19/9,5 žlutá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 19/9,5mm (3/4\") žlutá (cívka 100m)","100m",132.49162185332398,{"$f":"F4578*(1-Elteq!$F$9)","v":132.49162185332398},"8591735046446"]
["TECHNIK","PBF 25,4/12,7černá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 25,4/12,7mm (1\") černá (cívka 50m)","50m",89.626685371366221,{"$f":"F4579*(1-Elteq!$F$9)","v":89.626685371366221},"8591735056582"]
["TECHNIK","PBF 25,4/12,7hnědá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 25,4/12,7mm (1\") hnědá (cívka 50m)","50m",89.626685371366221,{"$f":"F4580*(1-Elteq!$F$9)","v":89.626685371366221},"8591735049522"]
["TECHNIK","PBF 25,4/12,7žlutá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 25,4/12,7mm (1\") žlutá (cívka 50m)","50m",89.626685371366221,{"$f":"F4581*(1-Elteq!$F$9)","v":89.626685371366221},"8591735038076"]
["TECHNIK","PBF 38/19 modrá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 38/19mm (1 1/2\") modrá (cívka 50m)","50m",144.55318406686189,{"$f":"F4582*(1-Elteq!$F$9)","v":144.55318406686189},"8591735038083"]
["TECHNIK","PBF 38/19 rudá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 38/19mm (1 1/2\") rudá (cívka 50m)","50m",144.55318406686189,{"$f":"F4583*(1-Elteq!$F$9)","v":144.55318406686189},"8591735038601"]
["TECHNIK","PBF 51/25,4 zelená R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 51/25,4mm (2\") zelená (cívka 30m)","30m",175.91324582206042,{"$f":"F4584*(1-Elteq!$F$9)","v":175.91324582206042},"8591735046651"]
["TECHNIK","PBF 51/25,4 žlutá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 51/25,4mm (2\") žlutá (cívka 30m)","30m",175.91324582206042,{"$f":"F4585*(1-Elteq!$F$9)","v":175.91324582206042},"8591735046668"]
["TECHNIK","PBF 76/38 modrá R",null,"Smršťovací trubice 2:1 tenkostěnná, rozměr před/po smrštění 76/38mm (3\") modrá (cívka 15m)","15m",115.23430976318514,{"$f":"F4586*(1-Elteq!$F$9)","v":115.23430976318514},"8591735041472"]
["TECHNIK","CFM   8/2 A",null,"Smršťovací trubice středněsilná s lepidlem, průměr 8,0/2,0mm černá","1,22m",3.7854749100949707,{"$f":"F4587*(1-Elteq!$F$9)","v":3.7854749100949707},"8591735045234"]
["TECHNIK","CFM   9/3 A",null,"Smršťovací trubice středněsilná s lepidlem, průměr 9,0/3,0mm černá","1,22m",3.9339249065692834,{"$f":"F4588*(1-Elteq!$F$9)","v":3.9339249065692834},"8591735016791"]
["TECHNIK","CFM  12/4 A",null,"Smršťovací trubice středněsilná s lepidlem, průměr 12,0/4,0mm černá","1,22m",4.7503998871780029,{"$f":"F4589*(1-Elteq!$F$9)","v":4.7503998871780029},"8591735045241"]
["TECHNIK","CFM  16/5 A",null,"Smršťovací trubice středněsilná s lepidlem, průměr 16,0/5,0mm černá","1,22m",5.8266623616167692,{"$f":"F4590*(1-Elteq!$F$9)","v":5.8266623616167692},"8591735048037"]
["TECHNIK","CFM  19/6 A",null,"Smršťovací trubice středněsilná s lepidlem, průměr 19,0/6,0mm černá","1,22m",5.3813123721938307,{"$f":"F4591*(1-Elteq!$F$9)","v":5.3813123721938307},"8591735016807"]
["TECHNIK","CFM  22/6 A",null,"Smršťovací trubice středněsilná s lepidlem, průměr 22,0/6,0mm černá","1,22m",7.0142623334112697,{"$f":"F4592*(1-Elteq!$F$9)","v":7.0142623334112697},"8591735048044"]
["TECHNIK","CFM  25/8 A",null,"Smršťovací trubice středněsilná s lepidlem, průměr 25,0/8,0mm černá","1,22m",6.1235623545653937,{"$f":"F4593*(1-Elteq!$F$9)","v":6.1235623545653937},"8591735016814"]
["TECHNIK","CFM  28/9 A",null,"Smršťovací trubice středněsilná s lepidlem, průměr 28,0/9,0mm černá","1,22m",6.3462373492768629,{"$f":"F4594*(1-Elteq!$F$9)","v":6.3462373492768629},"8591735016821"]
["TECHNIK","CFM  33/11 A",null,"Smršťovací trubice středněsilná s lepidlem, průměr 33,0/11,0mm černá","1,22m",7.236937328122738,{"$f":"F4595*(1-Elteq!$F$9)","v":7.236937328122738},"8591735016838"]
["TECHNIK","CFM  40/12 A",null,"Smršťovací trubice středněsilná s lepidlem, průměr 40,0/12,0mm černá","1,22m",8.4245372999172385,{"$f":"F4596*(1-Elteq!$F$9)","v":8.4245372999172385},"8591735016845"]
["TECHNIK","CFM  43/13 A",null,"Smršťovací trubice středněsilná s lepidlem, průměr 43,0/13,0mm černá","1,22m",9.3152372787631155,{"$f":"F4597*(1-Elteq!$F$9)","v":9.3152372787631155},"8591735016852"]
["TECHNIK","CFM  55/16 A",null,"Smršťovací trubice středněsilná s lepidlem, průměr 55,0/16,0mm černá","1,22m",11.913112217063585,{"$f":"F4598*(1-Elteq!$F$9)","v":11.913112217063585},"8591735016869"]
["TECHNIK","CFM  65/19 A",null,"Smršťovací trubice středněsilná s lepidlem, průměr 65,0/19,0mm černá","1,22m",13.954299668585383,{"$f":"F4599*(1-Elteq!$F$9)","v":13.954299668585383},"8591735045258"]
["TECHNIK","CFM  75/22 A",null,"Smršťovací trubice středněsilná s lepidlem, průměr 75,0/22,0mm černá","1,22m",14.585212153601212,{"$f":"F4600*(1-Elteq!$F$9)","v":14.585212153601212},"8591735016876"]
["TECHNIK","CFM  85/25 A",null,"Smršťovací trubice středněsilná s lepidlem, průměr 85,0/25,0mm černá","1,22m",15.438799633328509,{"$f":"F4601*(1-Elteq!$F$9)","v":15.438799633328509},"8591735045265"]
["TECHNIK","CFM  95/25 A",null,"Smršťovací trubice středněsilná s lepidlem, průměr 95,0/25,0mm černá","1,22m",19.818074529320729,{"$f":"F4602*(1-Elteq!$F$9)","v":19.818074529320729},"8591735016883"]
["TECHNIK","CFM 115/34 A",null,"Smršťovací trubice středněsilná s lepidlem, průměr 115,0/34,0mm černá","1,22m",21.451024490538167,{"$f":"F4603*(1-Elteq!$F$9)","v":21.451024490538167},"8591735016890"]
["TECHNIK","CFM 140/42 A",null,"Smršťovací trubice středněsilná s lepidlem, průměr 140,0/42,0mm černá","1,22m",28.168386831000813,{"$f":"F4604*(1-Elteq!$F$9)","v":28.168386831000813},"8591735045272"]
["TECHNIK","CFM 160/50 A",null,"Smršťovací trubice středněsilná s lepidlem, průměr 160,0/50,0mm černá","1,22m",43.124723975787802,{"$f":"F4605*(1-Elteq!$F$9)","v":43.124723975787802},"8591735016906"]
["TECHNIK","CFM 175/58 A",null,"Smršťovací trubice středněsilná s lepidlem, průměr 175,0/58,0mm černá","1,22m",48.3946988506259,{"$f":"F4606*(1-Elteq!$F$9)","v":48.3946988506259},"8591735016913"]
["TECHNIK","CFM 210/65 A",null,"Smršťovací trubice středněsilná s lepidlem, průměr 210,0/65,0mm černá","1,22m",67.470523397575064,{"$f":"F4607*(1-Elteq!$F$9)","v":67.470523397575064},"8591735048051"]
["TECHNIK","CFM 230/75 A",null,"Smršťovací trubice středněsilná s lepidlem, průměr 230,0/75,0mm černá","1,22m",77.416673161354012,{"$f":"F4608*(1-Elteq!$F$9)","v":77.416673161354012},"8591735016920"]
["TECHNIK","RPK   8/2",null,"Smršťovací trubice středněsilná s lepidlem, průměr 8,0/2,0mm, barva černá (CFM, TLS)","1m",3.0803374268419863,{"$f":"F4609*(1-Elteq!$F$9)","v":3.0803374268419863},"8591735037499"]
["TECHNIK","RPK   9/3",null,"Smršťovací trubice středněsilná s lepidlem, průměr 9,0/3,0mm, barva černá (CFM, TLS)","1m",3.2287874233162985,{"$f":"F4610*(1-Elteq!$F$9)","v":3.2287874233162985},"8591735018047"]
["TECHNIK","RPK   9/3 žz",null,"Smršťovací trubice středněsilná s lepidlem 9,0/3,0mm, žluto-zelená (RPKZ)","1m",3.4514624180277678,{"$f":"F4611*(1-Elteq!$F$9)","v":3.4514624180277678},"8591735027469"]
["TECHNIK","RPK  12/4",null,"Smršťovací trubice středněsilná s lepidlem 12,0/4,0mm, barva černá (CFM, TLS)","1m",3.8968124074507053,{"$f":"F4612*(1-Elteq!$F$9)","v":3.8968124074507053},"8591735018054"]
["TECHNIK","RPK  12/4 žz",null,"Smršťovací trubice středněsilná s lepidlem 12,0/4,0mm, žluto-zelená (RPKZ)","1m",3.9339249065692834,{"$f":"F4613*(1-Elteq!$F$9)","v":3.9339249065692834},"8591735027476"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"RPK  16/5",null,"Smršťovací trubice středněsilná s lepidlem 16,0/5,0mm, barva černá (CFM, TLS)","1m",4.7875123862965809,{"$f":"F4614*(1-Elteq!$F$9)","v":4.7875123862965809},"8591735032470"]
["TECHNIK","RPK  17/3",null,"Smršťovací trubice středněsilná s lepidlem 17,0/3,0mm, barva černá (CFM, TLS)","1m",5.2699748748380966,{"$f":"F4615*(1-Elteq!$F$9)","v":5.2699748748380966},"8591735038458"]
["TECHNIK","RPK  19/6",null,"Smršťovací trubice středněsilná s lepidlem 19,0/6,0mm, barva černá (CFM, TLS)","1m",4.4163873951107995,{"$f":"F4616*(1-Elteq!$F$9)","v":4.4163873951107995},"8591735037987"]
["TECHNIK","RPK  22/6",null,"Smršťovací trubice středněsilná s lepidlem 22,0/6,0mm, barva černá (CFM, TLS)","1m",5.7524373633796122,{"$f":"F4617*(1-Elteq!$F$9)","v":5.7524373633796122},"8591735018030"]
["TECHNIK","RPK  22/6 žz",null,"Smršťovací trubice středněsilná s lepidlem 22,0/6,0mm, žluto-zelená (RPKZ)","1m",6.1235623545653937,{"$f":"F4618*(1-Elteq!$F$9)","v":6.1235623545653937},"8591735050856"]
["TECHNIK","RPK  25/10 žz",null,"Smršťovací trubice středněsilná s lepidlem 25,0/10,0mm, žluto-zelená (RPKZ)","1m",6.6802498413440663,{"$f":"F4619*(1-Elteq!$F$9)","v":6.6802498413440663},"8591735027490"]
["TECHNIK","RPK  25/8",null,"Smršťovací trubice středněsilná s lepidlem 25,0/8,0mm, barva černá (CFM, TLS)","1m",5.0101873810080493,{"$f":"F4620*(1-Elteq!$F$9)","v":5.0101873810080493},"8591735018061"]
["TECHNIK","RPK  28/9",null,"Smršťovací trubice středněsilná s lepidlem 28,0/9,0mm, barva černá (CFM, TLS)","1m",5.1957498766009405,{"$f":"F4621*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735038861"]
["TECHNIK","RPK  33/11",null,"Smršťovací trubice středněsilná s lepidlem 33,0/11,0mm, barva černá (CFM, TLS)","1m",5.9379998589725034,{"$f":"F4622*(1-Elteq!$F$9)","v":5.9379998589725034},"8591735027513"]
["TECHNIK","RPK  33/8",null,"Smršťovací trubice středněsilná s lepidlem 33,0/8,0mm, barva černá (CFM, TLS)","1m",6.2720123510397068,{"$f":"F4623*(1-Elteq!$F$9)","v":6.2720123510397068},"8591735048686"]
["TECHNIK","RPK  35/12 žz",null,"Smršťovací trubice středněsilná s lepidlem 35,0/12,0mm, žluto-zelená (RPKZ)","1m",8.090524807850036,{"$f":"F4624*(1-Elteq!$F$9)","v":8.090524807850036},"8591735027506"]
["TECHNIK","RPK  40/12",null,"Smršťovací trubice středněsilná s lepidlem 40,0/12,0mm, barva černá (CFM, TLS)","1m",6.9029248360555355,{"$f":"F4625*(1-Elteq!$F$9)","v":6.9029248360555355},"8591735018078"]
["TECHNIK","RPK  40/16 žz",null,"Smršťovací trubice středněsilná s lepidlem 40,0/16,0mm, žluto-zelená (RPKZ)","1m",9.0183372858144892,{"$f":"F4626*(1-Elteq!$F$9)","v":9.0183372858144892},"8591735027520"]
["TECHNIK","RPK  55/16",null,"Smršťovací trubice středněsilná s lepidlem 55,0/16,0mm, barva černá (CFM, TLS)","1m",9.7605872681860522,{"$f":"F4627*(1-Elteq!$F$9)","v":9.7605872681860522},"8591735018016"]
["TECHNIK","RPK  65/19",null,"Smršťovací trubice středněsilná s lepidlem 65,0/19,0mm, barva černá (CFM, TLS)","1m",11.430649728522068,{"$f":"F4628*(1-Elteq!$F$9)","v":11.430649728522068},"8591735038854"]
["TECHNIK","RPK  75/22",null,"Smršťovací trubice středněsilná s lepidlem 75,0/22,0mm, barva černá (CFM, TLS)","1m",11.950224716182163,{"$f":"F4629*(1-Elteq!$F$9)","v":11.950224716182163},"8591735018085"]
["TECHNIK","RPK  85/25",null,"Smršťovací trubice středněsilná s lepidlem 85,0/25,0mm, barva černá (CFM, TLS)","1m",12.655362199435148,{"$f":"F4630*(1-Elteq!$F$9)","v":12.655362199435148},"8591735018023"]
["TECHNIK","RPK  95/25",null,"Smršťovací trubice středněsilná s lepidlem 95,0/25,0mm, barva černá (CFM, TLS)","1m",16.255274613937228,{"$f":"F4631*(1-Elteq!$F$9)","v":16.255274613937228},"8591735037505"]
["TECHNIK","RPK 115/34",null,"Smršťovací trubice středněsilná s lepidlem 115,0/34,0mm, barva černá (CFM, TLS)","1m",17.591324582206042,{"$f":"F4632*(1-Elteq!$F$9)","v":17.591324582206042},"8591735018092"]
["TECHNIK","RPK 140/42",null,"Smršťovací trubice středněsilná s lepidlem 140,0/42,0mm, barva černá (CFM, TLS)","1m",23.083974451755608,{"$f":"F4633*(1-Elteq!$F$9)","v":23.083974451755608},"8591735025281"]
["TECHNIK","RPK 160/50",null,"Smršťovací trubice středněsilná s lepidlem 160,0/50,0mm, barva černá (CFM, TLS)","1m",35.331099160886396,{"$f":"F4634*(1-Elteq!$F$9)","v":35.331099160886396},"8591735037451"]
["TECHNIK","RPK 175/58",null,"Smršťovací trubice středněsilná s lepidlem 175,0/58,0mm, barva černá (CFM, TLS)","1m",39.673261557760036,{"$f":"F4635*(1-Elteq!$F$9)","v":39.673261557760036},"8591735037468"]
["TECHNIK","RPK 210/65",null,"Smršťovací trubice středněsilná s lepidlem 210,0/65,0mm, barva černá (CFM, TLS)","1m",55.29762368668144,{"$f":"F4636*(1-Elteq!$F$9)","v":55.29762368668144},"8591735037475"]
["TECHNIK","RPK 230/75",null,"Smršťovací trubice středněsilná s lepidlem 230,0/75,0mm, barva černá (CFM, TLS)","1m",63.462373492768627,{"$f":"F4637*(1-Elteq!$F$9)","v":63.462373492768627},"8591735037482"]
["TECHNIK","RTE  4,8/2,8",null,"Smršťovací trubice teflonová rozměr 4,85/2,80mm, pracovní teplota -65°C až +260°C, transparentní","1,22m",12.840924695028038,{"$f":"F4638*(1-Elteq!$F$9)","v":12.840924695028038},""]
["TECHNIK","RTE  6,1/3,5",null,"Smršťovací trubice teflonová rozměr 6,10/3,55mm, pracovní teplota -65°C až +260°C, transparentní","1,22m",15.624362128921399,{"$f":"F4639*(1-Elteq!$F$9)","v":15.624362128921399},""]
["TECHNIK","RTE  7,7/4,4",null,"Smršťovací trubice teflonová rozměr 7,67/4,40mm, pracovní teplota -65°C až +260°C, transparentní","1,22m",18.482024561051915,{"$f":"F4640*(1-Elteq!$F$9)","v":18.482024561051915},""]
["TECHNIK","RTE 10,9/6,9",null,"Smršťovací trubice teflonová rozměr 10,92/6,90mm, pracovní teplota -65°C až +260°C, transparentní","1,22m",20.077862023150775,{"$f":"F4641*(1-Elteq!$F$9)","v":20.077862023150775},""]
["TECHNIK","RTE 11,9/8,5",null,"Smršťovací trubice teflonová rozměr 11,94/8,56mm, pracovní teplota -65°C až +260°C, transparentní","1,22m",21.00567450111523,{"$f":"F4642*(1-Elteq!$F$9)","v":21.00567450111523},""]
["TECHNIK","RTE 12,7/3,2",null,"Smršťovací trubice teflonová rozměr 12,70/3,20mm, pracovní teplota -65°C až +260°C, transparentní","1,22m",24.420024420024419,{"$f":"F4643*(1-Elteq!$F$9)","v":24.420024420024419},"8591735049287"]
["TECHNIK","CPA300  3/1",null,"Smršťovací trubice tenkostěnná s lepidlem 3:1, průměr 3,2/1,0 černá UL, CSA","1,22m",4.8988498836523151,{"$f":"F4644*(1-Elteq!$F$9)","v":4.8988498836523151},"8591735027636"]
["TECHNIK","CPA300  6,4/2,0",null,"Smršťovací trubice tenkostěnná s lepidlem 3:1, průměr 6,4/2,0 černá UL, CSA","1,22m",8.5358747972729727,{"$f":"F4645*(1-Elteq!$F$9)","v":8.5358747972729727},"8591735027643"]
["TECHNIK","CPA300 12,7/4,1",null,"Smršťovací trubice tenkostěnná s lepidlem 3:1, průměr 12,7/4,1 černá UL, CSA","1,22m",8.9441122875773331,{"$f":"F4646*(1-Elteq!$F$9)","v":8.9441122875773331},"8591735027650"]
["TECHNIK","CPA300 19/7,5",null,"Smršťovací trubice tenkostěnná s lepidlem 3:1, průměr 19,0/7,5 černá UL, CSA","1,22m",19.706737031964995,{"$f":"F4647*(1-Elteq!$F$9)","v":19.706737031964995},"8591735027667"]
["TECHNIK","HXKT  3,2/0,8",null,"Smršťovací trubice tenkostěnná s lepidlem 3:1","1,22m",4.6390623898222678,{"$f":"F4648*(1-Elteq!$F$9)","v":4.6390623898222678},""]
["TECHNIK","HXKT  4,8/1,5",null,"Smršťovací trubice tenkostěnná s lepidlem 3:1","1,22m",5.7153248642610341,{"$f":"F4649*(1-Elteq!$F$9)","v":5.7153248642610341},""]
["TECHNIK","HXKT  6,4/1,9",null,"Smršťovací trubice tenkostěnná s lepidlem 3:1","1,22m",7.1627123298855819,{"$f":"F4650*(1-Elteq!$F$9)","v":7.1627123298855819},""]
["TECHNIK","HXKT  9,5/3,4",null,"Smršťovací trubice tenkostěnná s lepidlem 3:1","1,22m",8.090524807850036,{"$f":"F4651*(1-Elteq!$F$9)","v":8.090524807850036},""]
["TECHNIK","HXKT 12,7/5",null,"Smršťovací trubice tenkostěnná s lepidlem 3:1","1,22m",8.9812247866959112,{"$f":"F4652*(1-Elteq!$F$9)","v":8.9812247866959112},""]
["TECHNIK","HXKT 19/8",null,"Smršťovací trubice tenkostěnná s lepidlem 3:1","1,22m",11.950224716182163,{"$f":"F4653*(1-Elteq!$F$9)","v":11.950224716182163},""]
["TECHNIK","HXKT 25,4/10,2",null,"Smršťovací trubice tenkostěnná s lepidlem 3:1","1,22m",17.851112076036088,{"$f":"F4654*(1-Elteq!$F$9)","v":17.851112076036088},""]
["TECHNIK","I3000  3,2/1,0 oranž",null,"Smršťovací trubice tenkostěnná 3:1, průměr 3,2/1,0 oranžová UL224,MIL,VG,DefStan 59/97,VDE, 24kV/mm","150m",165.52174606885853,{"$f":"F4655*(1-Elteq!$F$9)","v":165.52174606885853},""]
["TECHNIK","I3000  6,4/2,0 žlutá",null,"Smršťovací trubice tenkostěnná 3:1, průměr 6,4/2,0 žlutá UL224, MIL, VG, DefStan 59/97, VDE, 24kV/mm","75m",89.069997884587551,{"$f":"F4656*(1-Elteq!$F$9)","v":89.069997884587551},""]
["TECHNIK","I3000 12,7/4,0 oranž",null,"Smršťovací trubice tenkostěnná 3:1, průměr 12,7/4,0 oranžová UL224,MIL,VG,DefStan 59/97,VDE, 24kV/mm","50m",96.863622699488957,{"$f":"F4657*(1-Elteq!$F$9)","v":96.863622699488957},""]
["TECHNIK","I3000 25,4/8,0 žlutá",null,"Smršťovací trubice tenkostěnná 3:1, průměr 25,4/8,0 žlutá UL224, MIL,VG, DefStan 59/97, VDE, 24kV/mm","30m",125.81137201197991,{"$f":"F4658*(1-Elteq!$F$9)","v":125.81137201197991},""]
["TECHNIK","IAKT  3/1",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 3,0/1,0mm černá (balení 25ks)","1,22m",1.5216124638617039,{"$f":"F4659*(1-Elteq!$F$9)","v":1.5216124638617039},"8591735016678"]
["TECHNIK","IAKT  3/1 .",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 3,0/1,0mm černá","1,22m",1.5216124638617039,{"$f":"F4660*(1-Elteq!$F$9)","v":1.5216124638617039},""]
["TECHNIK","IAKT  3/1 R300",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 3,0/1,0mm černá (cívka)","300m",374.09399111526773,{"$f":"F4661*(1-Elteq!$F$9)","v":374.09399111526773},"8591735052935"]
["TECHNIK","IAKT  3/1 transp",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 3,0/1,0mm transparentní","1,22m",1.5216124638617039,{"$f":"F4662*(1-Elteq!$F$9)","v":1.5216124638617039},"8591735027544"]
["TECHNIK","IAKT  4,5/1,5",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 4,5/1,5mm černá (balení 25ks)","1,22m",1.6329499612174385,{"$f":"F4663*(1-Elteq!$F$9)","v":1.6329499612174385},"8591735046453"]
["TECHNIK","IAKT  4,5/1,5 .",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 4,5/1,5mm černá","1,22m",1.6329499612174385,{"$f":"F4664*(1-Elteq!$F$9)","v":1.6329499612174385},"8591735037109"]
["TECHNIK","IAKT  4,5/1,5 transp",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 4,5/1,5mm transparentní","1,22m",1.6329499612174385,{"$f":"F4665*(1-Elteq!$F$9)","v":1.6329499612174385},"8591735046682"]
["TECHNIK","IAKT  4,5/1,5.R100",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 4,5/1,5mm černá (cívka)","100m",133.9761218180671,{"$f":"F4666*(1-Elteq!$F$9)","v":133.9761218180671},"8591735027681"]
["TECHNIK","IAKT  4,5/1,5.R75",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 4,5/1,5mm černá (cívka)","75m",100.38931011575389,{"$f":"F4667*(1-Elteq!$F$9)","v":100.38931011575389},"8591735027698"]
["TECHNIK","IAKT  4/1",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 4,0/1,0mm černá (balení 25ks)","1,22m",2.5236499400633141,{"$f":"F4668*(1-Elteq!$F$9)","v":2.5236499400633141},"8591735016685"]
["TECHNIK","IAKT  4/1 .",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 4,0/1,0mm černá","1,22m",2.5236499400633141,{"$f":"F4669*(1-Elteq!$F$9)","v":2.5236499400633141},""]
["TECHNIK","IAKT  4/1 R300",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 4,0/1,0mm černá (cívka)","300m",620.5209852626266,{"$f":"F4670*(1-Elteq!$F$9)","v":620.5209852626266},"8591735027711"]
["TECHNIK","IAKT  4/1 transp",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 4,0/1,0mm transparentní","1,22m",2.5236499400633141,{"$f":"F4671*(1-Elteq!$F$9)","v":2.5236499400633141},"8591735027537"]
["TECHNIK","IAKT  6/2",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 6,0/2,0mm černá (balení 10ks)","1,22m",2.3751999435890014,{"$f":"F4672*(1-Elteq!$F$9)","v":2.3751999435890014},"8591735016692"]
["TECHNIK","IAKT  6/2 .",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 6,0/2,0mm černá","1,22m",2.3751999435890014,{"$f":"F4673*(1-Elteq!$F$9)","v":2.3751999435890014},""]
["TECHNIK","IAKT  6/2 R300",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 6,0/2,0mm černá (cívka)","300m",581.01472995090012,{"$f":"F4674*(1-Elteq!$F$9)","v":581.01472995090012},"8591735027735"]
["TECHNIK","IAKT  6/2 transp",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 6,0/2,0mm transparentní","1,22m",2.3751999435890014,{"$f":"F4675*(1-Elteq!$F$9)","v":2.3751999435890014},"8591735027551"]
["TECHNIK","IAKT  6/2 transpR300",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 6,0/2,0mm transparentní (cívka)","300m",583.96517363082717,{"$f":"F4676*(1-Elteq!$F$9)","v":583.96517363082717},"8591735052720"]
["TECHNIK","IAKT  8/2",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 8,0/2,0mm černá (balení 10ks)","1,22m",3.59991241450208,{"$f":"F4677*(1-Elteq!$F$9)","v":3.59991241450208},"8591735016708"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"IAKT  8/2 .",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 8,0/2,0mm černá","1,22m",3.59991241450208,{"$f":"F4678*(1-Elteq!$F$9)","v":3.59991241450208},""]
["TECHNIK","IAKT  8/2 transp",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 8,0/2,0mm transparentní","1,22m",3.59991241450208,{"$f":"F4679*(1-Elteq!$F$9)","v":3.59991241450208},"8591735027568"]
["TECHNIK","IAKT  9/3",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 9,0/3,0mm černá (balení 10ks)","1,22m",2.783437433893361,{"$f":"F4680*(1-Elteq!$F$9)","v":2.783437433893361},"8591735016715"]
["TECHNIK","IAKT  9/3 .",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 9,0/3,0mm černá","1,22m",2.783437433893361,{"$f":"F4681*(1-Elteq!$F$9)","v":2.783437433893361},""]
["TECHNIK","IAKT  9/3 R150",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 9,0/3,0mm černá (cívka)","150m",342.17724187329048,{"$f":"F4682*(1-Elteq!$F$9)","v":342.17724187329048},"8591735047177"]
["TECHNIK","IAKT  9/3 transp",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 9,0/3,0mm transparentní","1,22m",2.783437433893361,{"$f":"F4683*(1-Elteq!$F$9)","v":2.783437433893361},"8591735027575"]
["TECHNIK","IAKT  9/3 transpR150",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 9,0/3,0mm transparentní (cívka)","150m",342.17724187329048,{"$f":"F4684*(1-Elteq!$F$9)","v":342.17724187329048},"8591735054274"]
["TECHNIK","IAKT 12/3",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 12,0/3,0mm černá (balení 10ks)","1,22m",4.3792748959922214,{"$f":"F4685*(1-Elteq!$F$9)","v":4.3792748959922214},"8591735016722"]
["TECHNIK","IAKT 12/3 .",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 12,0/3,0mm černá","1,22m",4.3792748959922214,{"$f":"F4686*(1-Elteq!$F$9)","v":4.3792748959922214},""]
["TECHNIK","IAKT 12/3 R100",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 12,0/3,0mm černá (cívka)","100m",358.87786647665069,{"$f":"F4687*(1-Elteq!$F$9)","v":358.87786647665069},"8591735027766"]
["TECHNIK","IAKT 12/3 transp",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 12,0/3,0mm transparentní","1,22m",4.3792748959922214,{"$f":"F4688*(1-Elteq!$F$9)","v":4.3792748959922214},"8591735027582"]
["TECHNIK","IAKT 12/3 transpR100",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 12,0/3,0mm transparentní (cívka)","100m",358.87786647665069,{"$f":"F4689*(1-Elteq!$F$9)","v":358.87786647665069},""]
["TECHNIK","IAKT 12/4",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 12,0/4,0mm černá (balení 10ks)","1,22m",3.6741374127392366,{"$f":"F4690*(1-Elteq!$F$9)","v":3.6741374127392366},"8591735016739"]
["TECHNIK","IAKT 12/4 .",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 12,0/4,0mm černá","1,22m",3.6741374127392366,{"$f":"F4691*(1-Elteq!$F$9)","v":3.6741374127392366},""]
["TECHNIK","IAKT 12/4 transp",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 12,0/4,0mm transparentní","1,22m",3.6741374127392366,{"$f":"F4692*(1-Elteq!$F$9)","v":3.6741374127392366},"8591735027599"]
["TECHNIK","IAKT 12/4 transpR100",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 12,0/4,0mm transparentní (cívka)","100m",300.98236785166876,{"$f":"F4693*(1-Elteq!$F$9)","v":300.98236785166876},"8591735047047"]
["TECHNIK","IAKT 16/4",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 16,0/4,0mm černá (balení 10ks)","1,22m",5.4926498695495658,{"$f":"F4694*(1-Elteq!$F$9)","v":5.4926498695495658},"8591735016746"]
["TECHNIK","IAKT 16/4 .",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 16,0/4,0mm černá","1,22m",5.4926498695495658,{"$f":"F4695*(1-Elteq!$F$9)","v":5.4926498695495658},""]
["TECHNIK","IAKT 16/4 R50",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 16,0/4,0mm černá (cívka)","50m",225.08730715417644,{"$f":"F4696*(1-Elteq!$F$9)","v":225.08730715417644},"8591735027780"]
["TECHNIK","IAKT 16/4 transp",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 16,0/4,0mm transparentní","1,22m",5.4926498695495658,{"$f":"F4697*(1-Elteq!$F$9)","v":5.4926498695495658},"8591735027605"]
["TECHNIK","IAKT 16/4 transp R75",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 16,0/4,0mm transparentní (cívka)","75m",337.53817948346824,{"$f":"F4698*(1-Elteq!$F$9)","v":337.53817948346824},"8591735057107"]
["TECHNIK","IAKT 19/6",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 19,0/6,0mm černá (balení 10ks)","1,22m",5.6782123651424561,{"$f":"F4699*(1-Elteq!$F$9)","v":5.6782123651424561},"8591735015619"]
["TECHNIK","IAKT 19/6 .",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 19,0/6,0mm černá","1,22m",5.6782123651424561,{"$f":"F4700*(1-Elteq!$F$9)","v":5.6782123651424561},""]
["TECHNIK","IAKT 19/6 R50",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 19,0/6,0mm černá (cívka)","50m",232.69536947348499,{"$f":"F4701*(1-Elteq!$F$9)","v":232.69536947348499},"8591735027797"]
["TECHNIK","IAKT 19/6 transp",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 19,0/6,0mm transparentní","1,22m",5.6782123651424561,{"$f":"F4702*(1-Elteq!$F$9)","v":5.6782123651424561},"8591735027612"]
["TECHNIK","IAKT 24/6",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 24,0/6,0mm černá (balení 10ks)","1,22m",9.0183372858144892,{"$f":"F4703*(1-Elteq!$F$9)","v":9.0183372858144892},"8591735007874"]
["TECHNIK","IAKT 24/6 .",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 24,0/6,0mm černá","1,22m",9.0183372858144892,{"$f":"F4704*(1-Elteq!$F$9)","v":9.0183372858144892},""]
["TECHNIK","IAKT 24/6 transp",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 24,0/6,0mm transparentní","1,22m",9.0183372858144892,{"$f":"F4705*(1-Elteq!$F$9)","v":9.0183372858144892},"8591735045876"]
["TECHNIK","IAKT 24/8",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 24,0/8,0mm černá (balení 10ks)","1,22m",7.0142623334112697,{"$f":"F4706*(1-Elteq!$F$9)","v":7.0142623334112697},"8591735016753"]
["TECHNIK","IAKT 24/8 .",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 24,0/8,0mm černá","1,22m",7.0142623334112697,{"$f":"F4707*(1-Elteq!$F$9)","v":7.0142623334112697},""]
["TECHNIK","IAKT 24/8 transp",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 24,0/8,0mm transparentní","1,22m",7.0142623334112697,{"$f":"F4708*(1-Elteq!$F$9)","v":7.0142623334112697},"8591735048532"]
["TECHNIK","IAKT 32/8",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 32,0/8,0mm černá (balení 10ks)","1,22m",12.80381219590946,{"$f":"F4709*(1-Elteq!$F$9)","v":12.80381219590946},"8591735016760"]
["TECHNIK","IAKT 32/8 .",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 32,0/8,0mm černá","1,22m",12.80381219590946,{"$f":"F4710*(1-Elteq!$F$9)","v":12.80381219590946},""]
["TECHNIK","IAKT 32/8 R50",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 32,0/8,0mm černá (cívka)","50m",524.77073753669504,{"$f":"F4711*(1-Elteq!$F$9)","v":524.77073753669504},"8591735052744"]
["TECHNIK","IAKT 32/8 transp",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 32,0/8,0mm transparentní","1,22m",12.80381219590946,{"$f":"F4712*(1-Elteq!$F$9)","v":12.80381219590946},"8591735027629"]
["TECHNIK","IAKT 40/13",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 40,0/13,0mm černá (balení 10ks)","1,22m",13.508949679162445,{"$f":"F4713*(1-Elteq!$F$9)","v":13.508949679162445},"8591735016777"]
["TECHNIK","IAKT 40/13 .",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 40,0/13,0mm černá","1,22m",13.508949679162445,{"$f":"F4714*(1-Elteq!$F$9)","v":13.508949679162445},""]
["TECHNIK","IAKT 40/13 transp",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 40,0/13,0mm transparentní","1,22m",13.508949679162445,{"$f":"F4715*(1-Elteq!$F$9)","v":13.508949679162445},"8591735041878"]
["TECHNIK","IAKT 52/13",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 52,0/13,0mm černá (balení 10ks)","1,22m",18.148012068984713,{"$f":"F4716*(1-Elteq!$F$9)","v":18.148012068984713},"8591735016784"]
["TECHNIK","IAKT 52/13 .",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 52,0/13,0mm černá","1,22m",18.148012068984713,{"$f":"F4717*(1-Elteq!$F$9)","v":18.148012068984713},""]
["TECHNIK","IAKT 52/13 R30",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 52,0/13,0mm černá (cívka)","30m",446.2778019009022,{"$f":"F4718*(1-Elteq!$F$9)","v":446.2778019009022},"8591735048822"]
["TECHNIK","IAKT 52/13 transp",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 52,0/13,0mm transparentní","1,22m",18.148012068984713,{"$f":"F4719*(1-Elteq!$F$9)","v":18.148012068984713},"8591735048808"]
["TECHNIK","KY175  2,4/1,2 trans",null,"Smršťovací trubice tenkostěnná 2:1, průměr 2,4/1,2 transp. +175st. dle UL, CSA, MIL (balení 25ks)","1,22m",2.7463249347747829,{"$f":"F4720*(1-Elteq!$F$9)","v":2.7463249347747829},""]
["TECHNIK","KY175  3,2/1,6 trans",null,"Smršťovací trubice tenkostěnná 2:1, průměr 3,2/1,6 transp. +175st. dle UL, CSA, MIL (balení 25ks)","1,22m",3.0803374268419863,{"$f":"F4721*(1-Elteq!$F$9)","v":3.0803374268419863},""]
["TECHNIK","RCK  3/1 černá",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 3,0/1,0mm černá (po 10m)","1m",1.4844999647431258,{"$f":"F4722*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735017736"]
["TECHNIK","RCK  3/1 modrá",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 3,0/1,0mm modrá (po 10m)","1m",1.4844999647431258,{"$f":"F4723*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735024178"]
["TECHNIK","RCK  3/1 rudá",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 3,0/1,0mm rudá (po 10m)","1m",1.4844999647431258,{"$f":"F4724*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735024185"]
["TECHNIK","RCK  3/1 transp",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 3,0/1,0mm transparentní (po 10m)","1m",1.4844999647431258,{"$f":"F4725*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735024192"]
["TECHNIK","RCK  3/1 zelená",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 3,0/1,0mm zelená (po 10m)","1m",1.4844999647431258,{"$f":"F4726*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735024208"]
["TECHNIK","RCK  3/1 žlutá",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 3,0/1,0mm žlutá (po 10m)","1m",1.4844999647431258,{"$f":"F4727*(1-Elteq!$F$9)","v":1.4844999647431258},"8591735024215"]
["TECHNIK","RCK  4/1 černá",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 4,0/1,0mm černá (po 10m)","1m",1.6700624603360166,{"$f":"F4728*(1-Elteq!$F$9)","v":1.6700624603360166},"8591735017743"]
["TECHNIK","RCK  4/1 modrá",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 4,0/1,0mm modrá (po 10m)","1m",1.6700624603360166,{"$f":"F4729*(1-Elteq!$F$9)","v":1.6700624603360166},"8591735024147"]
["TECHNIK","RCK  4/1 rudá",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 4,0/1,0mm rudá (po 10m)","1m",1.6700624603360166,{"$f":"F4730*(1-Elteq!$F$9)","v":1.6700624603360166},"8591735024130"]
["TECHNIK","RCK  4/1 transp",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 4,0/1,0mm transparentní (po 10m)","1m",1.6700624603360166,{"$f":"F4731*(1-Elteq!$F$9)","v":1.6700624603360166},"8591735021191"]
["TECHNIK","RCK  4/1 zelená",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 4,0/1,0mm zelená (po 10m)","1m",1.6700624603360166,{"$f":"F4732*(1-Elteq!$F$9)","v":1.6700624603360166},"8591735024123"]
["TECHNIK","RCK  4/1 žlutá",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 4,0/1,0mm žlutá (po 10m)","1m",1.6700624603360166,{"$f":"F4733*(1-Elteq!$F$9)","v":1.6700624603360166},"8591735024116"]
["TECHNIK","RCK  6/2 černá",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 6,0/2,0mm černá (po 10m)","1m",1.6329499612174385,{"$f":"F4734*(1-Elteq!$F$9)","v":1.6329499612174385},"8591735017750"]
["TECHNIK","RCK  6/2 hnědá",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 6,0/2,0mm hnědá (po 10m)","1m",1.6329499612174385,{"$f":"F4735*(1-Elteq!$F$9)","v":1.6329499612174385},"8591735040321"]
["TECHNIK","RCK  6/2 modrá",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 6,0/2,0mm modrá (po 10m)","1m",1.6329499612174385,{"$f":"F4736*(1-Elteq!$F$9)","v":1.6329499612174385},"8591735024154"]
["TECHNIK","RCK  6/2 rudá",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 6,0/2,0mm rudá (po 10m)","1m",1.6329499612174385,{"$f":"F4737*(1-Elteq!$F$9)","v":1.6329499612174385},"8591735024161"]
["TECHNIK","RCK  6/2 transp",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 6,0/2,0mm transparentní (po 10m)","1m",1.6329499612174385,{"$f":"F4738*(1-Elteq!$F$9)","v":1.6329499612174385},"8591735021214"]
["TECHNIK","RCK  6/2 zelená",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 6,0/2,0mm zelená (po 10m)","1m",1.6329499612174385,{"$f":"F4739*(1-Elteq!$F$9)","v":1.6329499612174385},"8591735024222"]
["TECHNIK","RCK  6/2 žlutá",null,"Smršťovací trubice 3:1 tenkostěnná s lepidlem 6,0/2,0mm žlutá (po 10m)","1m",1.6329499612174385,{"$f":"F4740*(1-Elteq!$F$9)","v":1.6329499612174385},"8591735024239"]
["TECHNIK","RCK  8/2 černá",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 8,0/2,0mm černá (po 10m)","1m",1.781399957691751,{"$f":"F4741*(1-Elteq!$F$9)","v":1.781399957691751},"8591735017767"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"RCK  8/2 černá R",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 8,0/2,0mm černá (cívka 100m)","100m",178.1399957691751,{"$f":"F4742*(1-Elteq!$F$9)","v":178.1399957691751},"8591735037048"]
["TECHNIK","RCK  8/2 hnědá",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 8,0/2,0mm hnědá (po 10m)","1m",1.781399957691751,{"$f":"F4743*(1-Elteq!$F$9)","v":1.781399957691751},"8591735040314"]
["TECHNIK","RCK  8/2 modrá",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 8,0/2,0mm modrá (po 10m)","1m",1.781399957691751,{"$f":"F4744*(1-Elteq!$F$9)","v":1.781399957691751},"8591735024253"]
["TECHNIK","RCK  8/2 rudá",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 8,0/2,0mm rudá (po 10m)","1m",1.781399957691751,{"$f":"F4745*(1-Elteq!$F$9)","v":1.781399957691751},"8591735024260"]
["TECHNIK","RCK  8/2 transp",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 8,0/2,0mm transparentní (po 10m)","1m",1.781399957691751,{"$f":"F4746*(1-Elteq!$F$9)","v":1.781399957691751},"8591735021221"]
["TECHNIK","RCK  8/2 zelená",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 8,0/2,0mm zelená (po 10m)","1m",1.781399957691751,{"$f":"F4747*(1-Elteq!$F$9)","v":1.781399957691751},"8591735024277"]
["TECHNIK","RCK  8/2 žlutá",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 8,0/2,0mm žlutá (po 10m)","1m",1.781399957691751,{"$f":"F4748*(1-Elteq!$F$9)","v":1.781399957691751},"8591735024284"]
["TECHNIK","RCK 12/3 černá",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 12,0/3,0mm černá (po 10m)","1m",4.00814990480644,{"$f":"F4749*(1-Elteq!$F$9)","v":4.00814990480644},"8591735017774"]
["TECHNIK","RCK 12/3 modrá",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 12,0/3,0mm modrá (po 10m)","1m",4.00814990480644,{"$f":"F4750*(1-Elteq!$F$9)","v":4.00814990480644},"8591735024291"]
["TECHNIK","RCK 12/3 rudá",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 12,0/3,0mm rudá (po 10m)","1m",4.00814990480644,{"$f":"F4751*(1-Elteq!$F$9)","v":4.00814990480644},"8591735024307"]
["TECHNIK","RCK 12/3 transp",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 12,0/3,0mm transparentní (po 10m)","1m",4.00814990480644,{"$f":"F4752*(1-Elteq!$F$9)","v":4.00814990480644},"8591735024314"]
["TECHNIK","RCK 12/3 zelená",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 12,0/3,0mm zelená (po 10m)","1m",4.00814990480644,{"$f":"F4753*(1-Elteq!$F$9)","v":4.00814990480644},"8591735024321"]
["TECHNIK","RCK 12/3 žlutá",null,"Smršťovací trubice 4:1 tenkostěnná s lepidlem 12,0/3,0mm žlutá (po 10m)","1m",4.00814990480644,{"$f":"F4754*(1-Elteq!$F$9)","v":4.00814990480644},"8591735024338"]
["TECHNIK","SLV   1,5 CU/3",null,"Kabelový soubor Cu 3x1,5mm2 s Cu spojkami","1sada",3.3030124215534551,{"$f":"F4755*(1-Elteq!$F$9)","v":3.3030124215534551},"8591735041106"]
["TECHNIK","SLV   1,5 CU/5",null,"Kabelový soubor Cu 5x1,5mm2 s Cu spojkami","1sada",3.6741374127392366,{"$f":"F4756*(1-Elteq!$F$9)","v":3.6741374127392366},"8591735056872"]
["TECHNIK","SLV   2,5 CU/3",null,"Kabelový soubor Cu 3x2,5mm2 s Cu spojkami","1sada",3.3030124215534551,{"$f":"F4757*(1-Elteq!$F$9)","v":3.3030124215534551},"8591735041113"]
["TECHNIK","SLV   2,5 CU/5",null,"Kabelový soubor Cu 5x2,5mm2 s Cu spojkami","1sada",3.6741374127392366,{"$f":"F4758*(1-Elteq!$F$9)","v":3.6741374127392366},"8591735056889"]
["TECHNIK","SLV   4,0 CU/5",null,"Kabelový soubor Cu 5x4,0mm2 s Cu spojkami","1sada",5.0101873810080493,{"$f":"F4759*(1-Elteq!$F$9)","v":5.0101873810080493},"8591735056896"]
["TECHNIK","SLV   6,0 CU/5",null,"Kabelový soubor Cu 5x6,0mm2 s Cu spojkami","1sada",5.6039873669053,{"$f":"F4760*(1-Elteq!$F$9)","v":5.6039873669053},"8591735056902"]
["TECHNIK","SLV  10 AL",null,"Kabelový soubor Al 4x10mm2 s Al spojkami","1sada",8.4987622981543947,{"$f":"F4761*(1-Elteq!$F$9)","v":8.4987622981543947},"8591735056919"]
["TECHNIK","SLV  10 CU/5",null,"Kabelový soubor Cu 5x10mm2 s Cu spojkami","1sada",7.3482748254784731,{"$f":"F4762*(1-Elteq!$F$9)","v":7.3482748254784731},"8591735056926"]
["TECHNIK","SLV  16 AL",null,"Kabelový soubor Al 4x16mm2 s Al spojkami","1sada",8.7214372928658648,{"$f":"F4763*(1-Elteq!$F$9)","v":8.7214372928658648},"8591735038434"]
["TECHNIK","SLV  16 AL/5",null,"Kabelový soubor Al 5x16mm2 s Al spojkami","1sada",11.504874726759224,{"$f":"F4764*(1-Elteq!$F$9)","v":11.504874726759224},"8591735030117"]
["TECHNIK","SLV  16 CU",null,"Kabelový soubor Cu 4x16mm2 s Cu spojkami","1sada",9.5007997743560058,{"$f":"F4765*(1-Elteq!$F$9)","v":9.5007997743560058},"8591735036508"]
["TECHNIK","SLV  16 CU/5",null,"Kabelový soubor Cu 5x16mm2 s Cu spojkami","1sada",11.504874726759224,{"$f":"F4766*(1-Elteq!$F$9)","v":11.504874726759224},"8591735030032"]
["TECHNIK","SLV  25 AL",null,"Kabelový soubor Al 4x25mm2 s Al spojkami","1sada",9.5007997743560058,{"$f":"F4767*(1-Elteq!$F$9)","v":9.5007997743560058},"8591735041069"]
["TECHNIK","SLV  25 AL/5",null,"Kabelový soubor Al 5x25mm2 s Al spojkami","1sada",12.61824970031657,{"$f":"F4768*(1-Elteq!$F$9)","v":12.61824970031657},"8591735030049"]
["TECHNIK","SLV  25 CU",null,"Kabelový soubor Cu 4x25mm2 s Cu spojkami","1sada",11.764662220589273,{"$f":"F4769*(1-Elteq!$F$9)","v":11.764662220589273},"8591735030070"]
["TECHNIK","SLV  25 CU/5",null,"Kabelový soubor Cu 5x25mm2 s Cu spojkami","1sada",13.02648719062093,{"$f":"F4770*(1-Elteq!$F$9)","v":13.02648719062093},"8591735030087"]
["TECHNIK","SLV  35 AL",null,"Kabelový soubor Al 4x35mm2 s Al spojkami","1sada",15.327462135972775,{"$f":"F4771*(1-Elteq!$F$9)","v":15.327462135972775},"8591735038700"]
["TECHNIK","SLV  35 CU",null,"Kabelový soubor Cu 3x35mm2 + 1x25mm2 s Cu spojkami","1sada",14.882112146549836,{"$f":"F4772*(1-Elteq!$F$9)","v":14.882112146549836},"8591735038878"]
["TECHNIK","SLV  35 CU/5",null,"Kabelový soubor Cu 5x35mm2 s Cu spojkami","1sada",16.366612111292962,{"$f":"F4773*(1-Elteq!$F$9)","v":16.366612111292962},"8591735055516"]
["TECHNIK","SLV  50 AL",null,"Kabelový soubor Al 4x50mm2 s Al spojkami","1sada",15.550137130684243,{"$f":"F4774*(1-Elteq!$F$9)","v":15.550137130684243},"8591735041076"]
["TECHNIK","SLV  50 CU",null,"Kabelový soubor Cu 3x50mm2 + 1x35mm2 s Cu spojkami","1sada",16.40372461041154,{"$f":"F4775*(1-Elteq!$F$9)","v":16.40372461041154},"8591735041120"]
["TECHNIK","SLV  70 AL",null,"Kabelový soubor Al 4x70mm2 s Al spojkami","1sada",22.007711977316841,{"$f":"F4776*(1-Elteq!$F$9)","v":22.007711977316841},"8591735041083"]
["TECHNIK","SLV  70 CU",null,"Kabelový soubor Cu 3x70mm2 + 50mm2 s Cu spojkami","1sada",25.79318688741181,{"$f":"F4777*(1-Elteq!$F$9)","v":25.79318688741181},"8591735041137"]
["TECHNIK","SLV  95 AL",null,"Kabelový soubor Al 3x95mm2 + 70mm2 s Al spojkami","1sada",23.306649446467077,{"$f":"F4778*(1-Elteq!$F$9)","v":23.306649446467077},"8591735053239"]
["TECHNIK","SLV  95 CU",null,"Kabelový soubor Cu 3x95mm2 + 50mm2 s Cu spojkami","1sada",28.205499330119391,{"$f":"F4779*(1-Elteq!$F$9)","v":28.205499330119391},"8591735035464"]
["TECHNIK","SLV 120 AL",null,"Kabelový soubor Al 3x120mm2 + 70mm2 s Al spojkami","1sada",25.42206189622603,{"$f":"F4780*(1-Elteq!$F$9)","v":25.42206189622603},"8591735047276"]
["TECHNIK","SLV 120 CU",null,"Kabelový soubor Cu 3x120mm2 + 70mm2 s Cu spojkami","1sada",34.625961677633413,{"$f":"F4781*(1-Elteq!$F$9)","v":34.625961677633413},"8591735035457"]
["TECHNIK","SLV 150 AL",null,"Kabelový soubor Al 3x150mm2 + 70mm2 s Al spojkami","1sada",25.867411885648966,{"$f":"F4782*(1-Elteq!$F$9)","v":25.867411885648966},"8591735041090"]
["TECHNIK","SLV 150 CU",null,"Kabelový soubor Cu 3x150mm2 + 70mm2 s Cu spojkami","1sada",37.075386619459564,{"$f":"F4783*(1-Elteq!$F$9)","v":37.075386619459564},"8591735035440"]
["TECHNIK","SLV 185 AL",null,"Kabelový soubor Al 3x185mm2 + 95mm2 s Al spojkami, pro zkružené Al kabely","1sada",33.549699203194642,{"$f":"F4784*(1-Elteq!$F$9)","v":33.549699203194642},"8591735048563"]
["TECHNIK","SLV 185 CU",null,"Kabelový soubor Cu 3x185mm2 + 95mm2 s Cu spojkami","1sada",49.025611335641727,{"$f":"F4785*(1-Elteq!$F$9)","v":49.025611335641727},"8591735036515"]
["TECHNIK","SLV 240 AL",null,"Kabelový soubor Al 3x240mm2 + 120mm2 s Al spojkami","1sada",33.77237419790611,{"$f":"F4786*(1-Elteq!$F$9)","v":33.77237419790611},"8591735037611"]
["TECHNIK","SLV 240 CU",null,"Kabelový soubor Cu 3x240mm2 + 120mm2 s Cu spojkami","1sada",53.998686217531201,{"$f":"F4787*(1-Elteq!$F$9)","v":53.998686217531201},"8591735035433"]
["TECHNIK","SLV-SV  1,5-6",null,"Univerzální kabelový soubor Al+Cu 4x1,5 - 4x6,0mm2 se šroubovými spojovači s inbusovými šrouby","1sada",12.284237208249367,{"$f":"F4788*(1-Elteq!$F$9)","v":12.284237208249367},"8591735053994"]
["TECHNIK","SLV-SV  1,5-6/5",null,"Univerzální kabelový soubor Al+Cu 5x1,5 - 5x6,0mm2 se šroubovými spojovači s inbusovými šrouby","1sada",14.585212153601212,{"$f":"F4789*(1-Elteq!$F$9)","v":14.585212153601212},"8591735040758"]
["TECHNIK","SLV-SV  2,5",null,"Univerzální kabelový soubor Al+Cu 4x1,5-2,5mm2 s lisovacími spojkami","1sada",3.59991241450208,{"$f":"F4790*(1-Elteq!$F$9)","v":3.59991241450208},"8591735029678"]
["TECHNIK","SLV-SV  2,5/5",null,"Univerzální kabelový soubor Al+Cu 5x1,5-2,5mm2 s lisovacími spojkami","1sada",4.045262403925018,{"$f":"F4791*(1-Elteq!$F$9)","v":4.045262403925018},"8591735030094"]
["TECHNIK","SLV-SV  4",null,"Univerzální kabelový soubor Al+Cu 4x4,0-6,0mm2 s lisovacími spojkami","1sada",3.7854749100949707,{"$f":"F4792*(1-Elteq!$F$9)","v":3.7854749100949707},"8591735029685"]
["TECHNIK","SLV-SV  4/5",null,"Univerzální kabelový soubor Al+Cu 5x4,0-6,0mm2 s lisovacími spojkami","1sada",4.1565999012807522,{"$f":"F4793*(1-Elteq!$F$9)","v":4.1565999012807522},"8591735030100"]
["TECHNIK","SLV-SV  4-16",null,"Univerzální kabelový soubor Al+Cu 4x4,0 - 4x16mm2 se šroubovými spojovači s inbusovými šrouby","1sada",16.292387113055806,{"$f":"F4794*(1-Elteq!$F$9)","v":16.292387113055806},"8591735047054"]
["TECHNIK","SLV-SV  4-16/5",null,"Univerzální kabelový soubor Al+Cu 5x4,0 - 5x16mm2 se šroubovými spojovači s inbusovými šrouby","1sada",19.484062037253526,{"$f":"F4795*(1-Elteq!$F$9)","v":19.484062037253526},"8591735040765"]
["TECHNIK","SLV-SV  6",null,"Univerzální kabelový soubor Al+Cu 4x6,0mm2 s lisovacími spojkami","1sada",5.0101873810080493,{"$f":"F4796*(1-Elteq!$F$9)","v":5.0101873810080493},"8591735029692"]
["TECHNIK","SLV-SV  6/5",null,"Univerzální kabelový soubor Al+Cu 5x6,0mm2 s lisovacími spojkami","1sada",5.9008873598539253,{"$f":"F4797*(1-Elteq!$F$9)","v":5.9008873598539253},"8591735030124"]
["TECHNIK","SLV-SV  6-25",null,"Univerzální kabelový soubor Al+Cu 4x6 - 4x35mm2 se šroubovými spojovači s inbusovými šrouby","1sada",16.700624603360165,{"$f":"F4798*(1-Elteq!$F$9)","v":16.700624603360165},"8591735038465"]
["TECHNIK","SLV-SV  6-25/5",null,"Univerzální kabelový soubor Al+Cu 5x6 - 5x35mm2 se šroubovými spojovači s inbusovými šrouby","1sada",21.339686993182433,{"$f":"F4799*(1-Elteq!$F$9)","v":21.339686993182433},"8591735029708"]
["TECHNIK","SLV-SV  6-25/5T",null,"Univerzální kabelový soubor Al+Cu 5x6 - 5x35mm2 se šroubovými spojovači s trhacími šrouby","1sada",32.06519923845152,{"$f":"F4800*(1-Elteq!$F$9)","v":32.06519923845152},"8591735051280"]
["TECHNIK","SLV-SV  6-25/T",null,"Univerzální kabelový soubor Al+Cu 4x6 - 4x35mm2 se šroubovými spojovači s trhacími šrouby","1sada",26.758111864494843,{"$f":"F4801*(1-Elteq!$F$9)","v":26.758111864494843},"8591735054113"]
["TECHNIK","SLV-SV 10",null,"Univerzální kabelový soubor Al+Cu 4x10mm2 s lisovacími spojkami","1sada",5.9008873598539253,{"$f":"F4802*(1-Elteq!$F$9)","v":5.9008873598539253},"8591735029715"]
["TECHNIK","SLV-SV 10/5",null,"Univerzální kabelový soubor Al+Cu 5x10mm2 s lisovacími spojkami","1sada",6.6802498413440663,{"$f":"F4803*(1-Elteq!$F$9)","v":6.6802498413440663},"8591735030131"]
["TECHNIK","SLV-SV 16-50",null,"Univerzální kabelový soubor Al+Cu 4x16 - 4x50mm2 se šroubovými spojovači s trhacími šrouby","1sada",29.801336792218251,{"$f":"F4804*(1-Elteq!$F$9)","v":29.801336792218251},"8591735030001"]
["TECHNIK","SLV-SV 35- 95",null,"Univerzální kabelový soubor Al+Cu 4x35 - 4x95mm2 se šroubovými spojovači s trhacími šrouby","1sada",28.762186816898062,{"$f":"F4805*(1-Elteq!$F$9)","v":28.762186816898062},"8591735029722"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"SLV-SV 35-150",null,"Univerzální kabelový soubor Al+Cu 4x35 - 4x150mm2 se šroubovými spojovači s trhacími šrouby","1sada",50.844123792452059,{"$f":"F4806*(1-Elteq!$F$9)","v":50.844123792452059},"8591735037895"]
["TECHNIK","SLV-SV 35-185",null,"Univerzální kabelový soubor Al+Cu 4x35 - 4x185mm2 se šroubovými spojovači s trhacími šrouby","1sada",54.369811208716982,{"$f":"F4807*(1-Elteq!$F$9)","v":54.369811208716982},"8591735036744"]
["TECHNIK","SLV-SV 95-240",null,"Univerzální kabelový soubor Al+Cu 4x95 - 4x240mm2 se šroubovými spojovači s trhacími šrouby","1sada",95.007997743560054,{"$f":"F4808*(1-Elteq!$F$9)","v":95.007997743560054},"8591735055585"]
["TECHNIK","SLV-SV120-240",null,"Univerzální kabelový soubor Al+Cu 4x120 - 4x240mm2 se šroubovými spojovači s trhacími šrouby","1sada",147.18817150428092,{"$f":"F4809*(1-Elteq!$F$9)","v":147.18817150428092},"8591735049751"]
["TECHNIK","SLV-SV120-240 AL",null,"Univerzální kabelový soubor Al 4x120 - 4x240mm2 se šroubovými spojovači s trhacími šrouby","1sada",133.9761218180671,{"$f":"F4810*(1-Elteq!$F$9)","v":133.9761218180671},"8591735049744"]
["TECHNIK","SLV-SV150-240",null,"Univerzální kabelový soubor Al+Cu 4x150 - 4x240mm2 se šroubovými spojovači s trhacími šrouby","1sada",105.8077349870663,{"$f":"F4811*(1-Elteq!$F$9)","v":105.8077349870663},"8591735036751"]
["TECHNIK","SLV-SV150-240 AL",null,"Univerzální kabelový soubor Al 4x150 - 4x240mm2 se šroubovými spojovači s trhacími šrouby","1sada",96.678060203896067,{"$f":"F4812*(1-Elteq!$F$9)","v":96.678060203896067},"8591735035815"]
["TECHNIK","SLV-SV3x240/120 AL",null,"Univerzální kabelový soubor Al 3x240 + 1x120mm2 se šroubovými spojovači s trhacími šrouby","1sada",95.750247725931615,{"$f":"F4813*(1-Elteq!$F$9)","v":95.750247725931615},"8591735053031"]
["TECHNIK","SVCZV  3x1,5-2,5",null,"Spojka se smršťitelnou trubicí pro vícežilové kabely 3x1,5-2,5mm2 / průměr 9-24mm, délka 250mm","1sada",3.8968124074507053,{"$f":"F4814*(1-Elteq!$F$9)","v":3.8968124074507053},"8591735013264"]
["TECHNIK","SVCZV  4x1,5-2,5",null,"Spojka se smršťitelnou trubicí pro vícežilové kabely 4x1,5-2,5mm2 / průměr 9-24mm, délka 250mm","1sada",4.2679373986364864,{"$f":"F4815*(1-Elteq!$F$9)","v":4.2679373986364864},"8591735052034"]
["TECHNIK","SVCZV  5x1,5-2,5",null,"Spojka se smršťitelnou trubicí pro vícežilové kabely 5x1,5-2,5mm2 / průměr 9-24mm, délka 250mm","1sada",5.1586373774823624,{"$f":"F4816*(1-Elteq!$F$9)","v":5.1586373774823624},"8591735052799"]
["TECHNIK","SVCZV  4x4-6",null,"Spojka se smršťitelnou trubicí pro vícežilové kabely 4x4-6mm2 / průměr 11-31mm, délka 250mm","1sada",6.6802498413440663,{"$f":"F4817*(1-Elteq!$F$9)","v":6.6802498413440663},"8591735040529"]
["TECHNIK","SVCZV  5x4-6",null,"Spojka se smršťitelnou trubicí pro vícežilové kabely 5x4-6mm2 / průměr 11-31mm, délka 250mm","1sada",7.0884873316484258,{"$f":"F4818*(1-Elteq!$F$9)","v":7.0884873316484258},"8591735040529"]
["TECHNIK","SVCZV  7x1,5-2,5",null,"Spojka se smršťitelnou trubicí pro vícežilové kabely 7x1,5-2,5mm2 / průměr 9-24mm, délka 250mm","1sada",5.5668748677867219,{"$f":"F4819*(1-Elteq!$F$9)","v":5.5668748677867219},"8591735052805"]
["TECHNIK","SVCZV  7x4-6",null,"Spojka se smršťitelnou trubicí pro vícežilové kabely 7x4-6mm2 / průměr 11-31mm, délka 250mm","1sada",9.6121372717117399,{"$f":"F4820*(1-Elteq!$F$9)","v":9.6121372717117399},"8591735040536"]
["TECHNIK","SVCZV 12x0,5-1",null,"Spojka se smršťitelnou trubicí pro vícežilové kabely 12x0,5-1,0mm2 / průměr 11-31mm, délka 250mm","1sada",6.7173623404626444,{"$f":"F4821*(1-Elteq!$F$9)","v":6.7173623404626444},"8591735053000"]
["TECHNIK","SVCZV 12x1,5-2,5",null,"Spojka se smršťitelnou trubicí pro vícežilové kabely 12x1,5-2,5mm2 / průměr 11-31mm, délka 250mm","1sada",7.5338373210713634,{"$f":"F4822*(1-Elteq!$F$9)","v":7.5338373210713634},"8591735052041"]
["TECHNIK","SVCZV 12x4-6",null,"Spojka se smršťitelnou trubicí pro vícežilové kabely 12x4-6mm2 / průměr 15-39mm, délka 333mm","1sada",15.772812125395712,{"$f":"F4823*(1-Elteq!$F$9)","v":15.772812125395712},"8591735040543"]
["TECHNIK","SVCZV 19x1,5-2,5",null,"Spojka se smršťitelnou trubicí pro vícežilové kabely 19x1,5-2,5mm2 / průměr 15-39mm, délka 250mm","1sada",14.919224645668415,{"$f":"F4824*(1-Elteq!$F$9)","v":14.919224645668415},"8591735056391"]
["TECHNIK","SVCZV 24x0,5-1",null,"Spojka se smršťitelnou trubicí pro vícežilové kabely 24x0,5-1,0mm2 / průměr 15-39mm, délka 250mm","1sada",11.059524737336288,{"$f":"F4825*(1-Elteq!$F$9)","v":11.059524737336288},"8591735053017"]
["TECHNIK","SVCZV 37x1,5-2,5",null,"Spojka se smršťitelnou trubicí pro vícežilové kabely 37x1,5-2,5mm2 / průměr 15-39mm, délka 333mm","1sada",27.38902434951067,{"$f":"F4826*(1-Elteq!$F$9)","v":27.38902434951067},"8591735056407"]
["TECHNIK","Brašna M",null,"10503820 malá lehká a pevná brašna se zipem","1ks",40.897974028673119,{"$f":"F4827*(1-Elteq!$F$9)","v":40.897974028673119},""]
["TECHNIK","Brašna V",null,"10506531 profesionální brašna se dvěmi objemnými kapsami","1ks",72.888948268887475,{"$f":"F4828*(1-Elteq!$F$9)","v":72.888948268887475},""]
["TECHNIK","Organizér M",null,"10503819 pevný otevřený organizér na nářadí a příslušenství","1ks",45.833936411444007,{"$f":"F4829*(1-Elteq!$F$9)","v":45.833936411444007},""]
["TECHNIK","Organizér V",null,"10503818 velký otevřený organizér na nářadí a příslušenství","1ks",64.761310961918866,{"$f":"F4830*(1-Elteq!$F$9)","v":64.761310961918866},""]
["TECHNIK","Pouzdro E",null,"10506535 pouzdro na opasek IRWIN pro elektrikáře","1ks",22.824186957925559,{"$f":"F4831*(1-Elteq!$F$9)","v":22.824186957925559},""]
["TECHNIK","Pouzdro V",null,"10506536 pouzdro na opasek IRWIN pro akkuvrtačku","1ks",20.226312019625091,{"$f":"F4832*(1-Elteq!$F$9)","v":20.226312019625091},""]
["TECHNIK","C1-BP 051",null,"Čelisti k LK-1 na mosazné objímky s bočním připojením typu A, pro průřezy 0,5-1mm2","1pár",175.91324582206042,{"$f":"F4833*(1-Elteq!$F$9)","v":175.91324582206042},"8591735023652"]
["TECHNIK","C1-BP 1525",null,"974915 KNIPEX čelisti k LK-1 na mosazné objímky s bočním připojením typu A, pro průřezy 1,5-2,5mm2","1pár",179.62449573391822,{"$f":"F4834*(1-Elteq!$F$9)","v":179.62449573391822},"8591735023669"]
["TECHNIK","C1-D 0256",null,"974908 KNIPEX čelisti k LK-1 na dutinky, pro průřezy 0,25-6mm2","1pár",55.854311173460111,{"$f":"F4835*(1-Elteq!$F$9)","v":55.854311173460111},"8591735023676"]
["TECHNIK","C1-D 1025",null,"974909 KNIPEX čelisti k LK-1 na dutinky, pro průřezy 10-25mm2","1pár",55.854311173460111,{"$f":"F4836*(1-Elteq!$F$9)","v":55.854311173460111},"8591735023683"]
["TECHNIK","C1-D 3550",null,"974919 KNIPEX čelisti k LK-1 na dutinky, pro průřezy 35 a 50mm2","1pár",86.100997955101292,{"$f":"F4837*(1-Elteq!$F$9)","v":86.100997955101292},"8591735023690"]
["TECHNIK","C1-DD 616",null,"974918 KNIPEX čelisti k LK-1 na dutinky dvojité, pro průřezy 2x6 - 2x16mm2","1pár",92.038997814073795,{"$f":"F4838*(1-Elteq!$F$9)","v":92.038997814073795},"8591735050580"]
["TECHNIK","C1-DSK 08056",null,"974924 KNIPEX čelisti k LK-1 na D-Sub konektory, pro průřezy 0,03-0,56mm2","1pár",135.831746773996,{"$f":"F4839*(1-Elteq!$F$9)","v":135.831746773996},"8591735016616"]
["TECHNIK","C1-H&S 4",null,"974962 KNIPEX čelisti k LK-1 na solární konektory Huber & Suhner, průřez 2,5-4,0mm2","1pár",112.26530983369889,{"$f":"F4840*(1-Elteq!$F$9)","v":112.26530983369889},"8591735032555"]
["TECHNIK","C1-H&S 6",null,"974963 KNIPEX čelisti k LK-1 na solární konektory Huber & Suhner, průřez 4,0-6,0mm2","1pár",112.26530983369889,{"$f":"F4841*(1-Elteq!$F$9)","v":112.26530983369889},"8591735032579"]
["TECHNIK","C1-HIR",null,"974967 KNIPEX čelisti k LK-1 na solární konektory Hirschmann SunCon, pro průřezy 2,5-6mm2","1pár",110.59524737336288,{"$f":"F4842*(1-Elteq!$F$9)","v":110.59524737336288},"8591735032562"]
["TECHNIK","C1-KK 01415",null,"974944 KNIPEX čelisti k LK-1 na stáčené kontakty, pro průřezy 0,14-1,5mm2","1pár",125.25468452520124,{"$f":"F4843*(1-Elteq!$F$9)","v":125.25468452520124},"8591735016623"]
["TECHNIK","C1-MC 3",null,"974965 KNIPEX čelisti k LK-1 na solární konektory Multi-Contact MC3 pro průřezy 2,5-6mm2","1pár",138.80074670348228,{"$f":"F4844*(1-Elteq!$F$9)","v":138.80074670348228},"8591735032586"]
["TECHNIK","C1-MC 4",null,"974966 KNIPEX čelisti k LK-1 na solární konektory Multi-Contact MC4, pro průřezy 2,5-6mm2","1pár",146.59437151838367,{"$f":"F4845*(1-Elteq!$F$9)","v":146.59437151838367},"8591735032593"]
["TECHNIK","C1-MC 4/4 UNI",null,"9749664 KNIPEX čelisti k LK-1 multifunkční na solární konektory Multi-Contact MC4, pro průřezy 4mm2","1pár",212.46905745385988,{"$f":"F4846*(1-Elteq!$F$9)","v":212.46905745385988},"8591735032609"]
["TECHNIK","C1-MC 4/6 UNI",null,"9749666 KNIPEX čelisti k LK-1 multifunkční na solární konektory Multi-Contact MC4, pro průřezy 6mm2","1pár",212.46905745385988,{"$f":"F4847*(1-Elteq!$F$9)","v":212.46905745385988},"8591735032616"]
["TECHNIK","C1-MK 0525",null,"974954 KNIPEX čelisti k LK-1 na modulové konektory, pro průřezy 0,5-2,5mm2","1pár",125.06912202960835,{"$f":"F4848*(1-Elteq!$F$9)","v":125.06912202960835},"8591735016630"]
["TECHNIK","C1-MO 0125",null,"974904 KNIPEX čelisti k LK-1 na mosazné objímky, pro průřezy 0,1-2,5mm2, šíře 2,8 a 4,8mm","1pár",73.111623263598943,{"$f":"F4849*(1-Elteq!$F$9)","v":73.111623263598943},"8591735023706"]
["TECHNIK","C1-MO 054",null,"Čelisti k LK-1 na mosazné objímky, pro průřezy 0,5-4mm2, šíře 4,8 a 6,3mm","1pár",145.48099654482633,{"$f":"F4850*(1-Elteq!$F$9)","v":145.48099654482633},"8591735055059"]
["TECHNIK","C1-MO 056",null,"974905 KNIPEX čelisti k LK-1 na mosazné objímky, pro průřezy 0,5-6mm2, šíře 4,8 a 6,3mm","1pár",73.111623263598943,{"$f":"F4851*(1-Elteq!$F$9)","v":73.111623263598943},"8591735023713"]
["TECHNIK","C1-OI 056",null,"974906 KNIPEX čelisti k LK-1 na oka izolovaná, pro průřezy 0,5-6mm2","1pár",51.58637377482362,{"$f":"F4852*(1-Elteq!$F$9)","v":51.58637377482362},"8591735023720"]
["TECHNIK","C1-OI 1016",null,"974916 KNIPEX čelisti k LK-1 na oka izolovaná, pro průřezy 10-16mm2","1pár",67.17362340462644,{"$f":"F4853*(1-Elteq!$F$9)","v":67.17362340462644},"8591735023737"]
["TECHNIK","C1-OL 1510",null,"974930 KNIPEX čelisti k LK-1 na oka lehčená, pro průřezy 1,5-10mm2","1pár",59.194436094132143,{"$f":"F4854*(1-Elteq!$F$9)","v":59.194436094132143},"8591735023744"]
["TECHNIK","C1-ON 02525",null,"Čelisti k LK-1 na oka neizolovaná, pro průřezy 0,25-2,5mm2","1pár",58.637748607353473,{"$f":"F4855*(1-Elteq!$F$9)","v":58.637748607353473},"8591735023751"]
["TECHNIK","C1-ON 0510",null,"974913 KNIPEX čelisti k LK-1 na oka neizolovaná, pro průřezy 0,5-10mm2 (CL-HN1)","1pár",58.637748607353473,{"$f":"F4856*(1-Elteq!$F$9)","v":58.637748607353473},"8591735023768"]
["TECHNIK","C1-ON 1625",null,"974923 KNIPEX čelisti k LK-1 na oka neizolovaná, pro průřezy 16-25mm2","1pár",58.637748607353473,{"$f":"F4857*(1-Elteq!$F$9)","v":58.637748607353473},"8591735023775"]
["TECHNIK","C1-ON 410",null,"Čelisti k LK-1 na oka neizolovaná, pro průřezy 4-10mm2","1pár",58.637748607353473,{"$f":"F4858*(1-Elteq!$F$9)","v":58.637748607353473},"8591735054021"]
["TECHNIK","C1-SIS 056",null,"Čelisti k LK-1 na oka a spojky se smršťovací bužírkou, pro průřezy 0,5-6mm2","1pár",55.11206119108855,{"$f":"F4859*(1-Elteq!$F$9)","v":55.11206119108855},"8591735036492"]
["TECHNIK","C1-SK 0144",null,"974960 KNIPEX čelisti k LK-1 na soustružené kontakty HTS a Harting, pro průřezy 0,14-4mm2","1pár",140.2852466682254,{"$f":"F4860*(1-Elteq!$F$9)","v":140.2852466682254},"8591735016647"]
["TECHNIK","C1-SK 156",null,"Čelisti k LK-1 na soustružené kontakty, pro průřezy 1,5-6mm2","1pár",140.2852466682254,{"$f":"F4861*(1-Elteq!$F$9)","v":140.2852466682254},"8591735010713"]
["TECHNIK","C1-SK 410",null,"Čelisti k LK-1 na soustružené kontakty, pro průřezy 4-10mm2","1pár",140.2852466682254,{"$f":"F4862*(1-Elteq!$F$9)","v":140.2852466682254},"8591735023782"]
["TECHNIK","C1-T 468W",null,"974970 KNIPEX čelisti k LK-1 na nestíněné RJ konektory Western","1pár",143.62537158889742,{"$f":"F4863*(1-Elteq!$F$9)","v":143.62537158889742},"8591735052508"]
["TECHNIK","C1-TYCO",null,"974968 KNIPEX čelisti k LK-1 na solární konektory Tyco Solarlok, pro průřezy 1,5-6mm2","1pár",189.45930800034142,{"$f":"F4864*(1-Elteq!$F$9)","v":189.45930800034142},"8591735032623"]
["TECHNIK","C1-X 1",null,"974940 KNIPEX čelisti k LK-1 na koaxiální koncovky RG 58, 59, 62, 71, 223","1pár",82.760873034429267,{"$f":"F4865*(1-Elteq!$F$9)","v":82.760873034429267},"8591735023799"]
["TECHNIK","C1-X 2",null,"974950 KNIPEX čelisti k LK-1 na koaxiální koncovky RG 58, 174, 188, 316","1pár",101.68824758490412,{"$f":"F4866*(1-Elteq!$F$9)","v":101.68824758490412},"8591735023805"]
["TECHNIK","C1-X 5",null,"Čelisti k LK-1 na koaxiální konektory RG 213, 11","1pár",111.89418484251311,{"$f":"F4867*(1-Elteq!$F$9)","v":111.89418484251311},"8591735041427"]
["TECHNIK","C2-BP 0525",null,"Čelisti ke kleštím LK-2 na izolované konektory s bočním připojením, pro průřezy 0,5-2,5mm2","1pár",24.123124427075794,{"$f":"F4868*(1-Elteq!$F$9)","v":24.123124427075794},"8591735035778"]
["TECHNIK","C2-D 02516",null,"Čelisti ke kleštím LK-2 na dutinky, pro průřezy 0,25-16mm2","1pár",32.102311737570098,{"$f":"F4869*(1-Elteq!$F$9)","v":32.102311737570098},"8591735036478"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"C2-D 0516",null,"Čelisti ke kleštím LK-2 na dutinky, pro průřezy 0,5-16mm2","1pár",23.009749453518449,{"$f":"F4870*(1-Elteq!$F$9)","v":23.009749453518449},"8591735010744"]
["TECHNIK","C2-D 054",null,"Čelisti ke kleštím LK-2 na dutinky, pro průřezy 0,5-4mm2","1pár",9.0925622840516453,{"$f":"F4871*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735008277"]
["TECHNIK","C2-D 056",null,"Čelisti ke kleštím LK-2 na dutinky, pro průřezy 0,5-6mm2","1pár",9.0925622840516453,{"$f":"F4872*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735033521"]
["TECHNIK","C2-D 1635",null,"Čelisti ke kleštím LK-2 na dutinky, pro průřezy 16-35mm2, široký trapéz","1pár",23.009749453518449,{"$f":"F4873*(1-Elteq!$F$9)","v":23.009749453518449},"8591735041526"]
["TECHNIK","C2-D 25/50",null,"Čelisti ke kleštím LK-2 na dutinky, pro průřezy 25 a 50mm2","1pár",23.009749453518449,{"$f":"F4874*(1-Elteq!$F$9)","v":23.009749453518449},"8591735023812"]
["TECHNIK","C2-D 35",null,"Čelisti ke kleštím LK-2 na dutinky, pro průřezy 16-35mm2","1pár",23.009749453518449,{"$f":"F4875*(1-Elteq!$F$9)","v":23.009749453518449},"8591735023829"]
["TECHNIK","C2-D 50",null,"Čelisti ke kleštím LK-2 na dutinky, pro průřezy 25-50mm2","1pár",32.102311737570098,{"$f":"F4876*(1-Elteq!$F$9)","v":32.102311737570098},"8591735033538"]
["TECHNIK","C2-D 616",null,"Čelisti ke kleštím LK-2 na dutinky, pro průřezy 6-16mm2","1pár",9.0925622840516453,{"$f":"F4877*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735008284"]
["TECHNIK","C2-DSK 05075",null,"Čelisti ke kleštím LK-2 na D-Sub-konektory, pro průřezy 0,05-0,75mm2","1pár",24.123124427075794,{"$f":"F4878*(1-Elteq!$F$9)","v":24.123124427075794},"8591735023843"]
["TECHNIK","C2-DSK 0805",null,"Čelisti ke kleštím LK-2 na D-Sub-konektory, pro průřezy 0,08-0,5mm2","1pár",24.123124427075794,{"$f":"F4879*(1-Elteq!$F$9)","v":24.123124427075794},"8591735023836"]
["TECHNIK","C2-FO SMA",null,"Čelisti ke kleštím LK-2 na fiber optic SMA (šestihran 3,83/4,52/5,46mm)","1pár",32.102311737570098,{"$f":"F4880*(1-Elteq!$F$9)","v":32.102311737570098},"8591735033545"]
["TECHNIK","C2-FO ST",null,"Čelisti ke kleštím LK-2 na fiber optic SMA, SMB, SFR, ST, SC (šestihran 3,25/3,83/4,52/5,00/5,46mm)","1pár",32.102311737570098,{"$f":"F4881*(1-Elteq!$F$9)","v":32.102311737570098},"8591735033552"]
["TECHNIK","C2-KK 02515",null,"Čelisti ke kleštím LK-2 na kruhové kontakty, pro průřezy 0,25-1,5mm2","1pár",9.0925622840516453,{"$f":"F4882*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735008291"]
["TECHNIK","C2-MC 3H",null,"Čelisti ke kleštím LK-2 na solární Multi-Contact MC3, pro průřezy 2,5-6mm2","1pár",32.102311737570098,{"$f":"F4883*(1-Elteq!$F$9)","v":32.102311737570098},"8591735054946"]
["TECHNIK","C2-MC 3T",null,"Čelisti ke kleštím LK-2 na solární Multi-Contact MC3, pro průřezy 4-6mm2","1pár",32.102311737570098,{"$f":"F4884*(1-Elteq!$F$9)","v":32.102311737570098},"8591735033569"]
["TECHNIK","C2-MC 4H",null,"Čelisti ke kleštím LK-2 na solární Multi-Contact MC4, pro průřezy 2,5-6mm2","1pár",32.102311737570098,{"$f":"F4885*(1-Elteq!$F$9)","v":32.102311737570098},"8591735033576"]
["TECHNIK","C2-MC 4T",null,"Čelisti ke kleštím LK-2 na solární Multi-Contact MC4, pro průřezy 4-6mm2","1pár",32.102311737570098,{"$f":"F4886*(1-Elteq!$F$9)","v":32.102311737570098},"8591735054939"]
["TECHNIK","C2-MO 0525",null,"Čelisti ke kleštím LK-2 na mosazné objímky, pro průřezy 0,5-2,5mm2 / 4,8mm","1pár",23.009749453518449,{"$f":"F4887*(1-Elteq!$F$9)","v":23.009749453518449},"8591735035785"]
["TECHNIK","C2-MO 0525 BP",null,"Čelisti ke kleštím LK-2 na mosazné objímky s bočním připojením typu A, pro průřezy 0,5-2,5mm2","1pár",32.102311737570098,{"$f":"F4888*(1-Elteq!$F$9)","v":32.102311737570098},"8591735033583"]
["TECHNIK","C2-MO 0525 BP-B",null,"Čelisti ke kleštím LK-2 na mosazné objímky s bočním připojením typu B, pro průřezy 0,5-2,5mm2","1pár",32.102311737570098,{"$f":"F4889*(1-Elteq!$F$9)","v":32.102311737570098},"8591735037550"]
["TECHNIK","C2-MO 056",null,"Čelisti ke kleštím LK-2 na mosazné objímky, pro průřezy 0,5-6mm2 / 6,3mm","1pár",9.0925622840516453,{"$f":"F4890*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735008307"]
["TECHNIK","C2-OI 056",null,"Čelisti ke kleštím LK-2 na oka a spojky izolované, pro průřezy 0,5-6mm2","1pár",9.0925622840516453,{"$f":"F4891*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735008314"]
["TECHNIK","C2-OL 056",null,"Čelisti ke kleštím LK-2 na oka lehčená, pro průřezy 0,5-6mm2","1pár",32.102311737570098,{"$f":"F4892*(1-Elteq!$F$9)","v":32.102311737570098},"8591735033590"]
["TECHNIK","C2-ON 0510",null,"Čelisti ke kleštím LK-2 na oka neizolovaná, pro průřezy 0,5-10mm2","1pár",9.0925622840516453,{"$f":"F4893*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735008321"]
["TECHNIK","C2-ON 07510",null,"Čelisti ke kleštím LK-2 na oka neizolovaná, pro průřezy 0,75-10mm2","1pár",9.0925622840516453,{"$f":"F4894*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735041533"]
["TECHNIK","C2-ON 1025",null,"Čelisti ke kleštím LK-2 na oka neizolovaná, pro průřezy 10-25mm2","1pár",32.102311737570098,{"$f":"F4895*(1-Elteq!$F$9)","v":32.102311737570098},"8591735035761"]
["TECHNIK","C2-SIS 056",null,"Čelisti ke kleštím LK-2 na oka a spojky se smršťovací bužírkou, pro průřezy 0,5-6mm2","1pár",32.102311737570098,{"$f":"F4896*(1-Elteq!$F$9)","v":32.102311737570098},"8591735036485"]
["TECHNIK","C2-SK 156",null,"Čelisti ke kleštím LK-2 na soustružené kontakty pro průřezy 0,5-6mm2","1pár",32.102311737570098,{"$f":"F4897*(1-Elteq!$F$9)","v":32.102311737570098},"8591735053963"]
["TECHNIK","C2-T10",null,"Čelisti ke kleštím LK-2 na PC konektory nestíněné RJ50-10p10c AMP","1pár",23.009749453518449,{"$f":"F4898*(1-Elteq!$F$9)","v":23.009749453518449},"8591735033606"]
["TECHNIK","C2-T4",null,"Čelisti ke kleštím LK-2 na PC konektory nestíněné RJ22-4p4c Stewart + AMP","1pár",23.009749453518449,{"$f":"F4899*(1-Elteq!$F$9)","v":23.009749453518449},"8591735033613"]
["TECHNIK","C2-T6",null,"Čelisti ke kleštím LK-2 na PC konektory nestíněné RJ11 a RJ12-6p6c Stewart","1pár",23.009749453518449,{"$f":"F4900*(1-Elteq!$F$9)","v":23.009749453518449},"8591735033620"]
["TECHNIK","C2-T68",null,"Čelisti ke kleštím LK-2 na PC konektory nestíněné RJ11, RJ12-6p6c a RJ45-8p8c","1pár",24.123124427075794,{"$f":"F4901*(1-Elteq!$F$9)","v":24.123124427075794},"8591735041540"]
["TECHNIK","C2-T6A",null,"Čelisti ke kleštím LK-2 na PC konektory nestíněné RJ11 a RJ12-6p6c AMP","1pár",32.102311737570098,{"$f":"F4902*(1-Elteq!$F$9)","v":32.102311737570098},"8591735036003"]
["TECHNIK","C2-T6DEC",null,"Čelisti ke kleštím LK-2 na PC konektory nestíněné RJ11 DEC MMJ-6p6c AMP","1pár",24.123124427075794,{"$f":"F4903*(1-Elteq!$F$9)","v":24.123124427075794},"8591735036010"]
["TECHNIK","C2-T8",null,"Čelisti ke kleštím LK-2 na PC konektory nestíněné RJ45-8p8c Stewart","1pár",24.123124427075794,{"$f":"F4904*(1-Elteq!$F$9)","v":24.123124427075794},"8591735023867"]
["TECHNIK","C2-T8A",null,"Čelisti ke kleštím LK-2 na PC konektory nestíněné RJ45-8p8c AMP","1pár",24.123124427075794,{"$f":"F4905*(1-Elteq!$F$9)","v":24.123124427075794},"8591735036027"]
["TECHNIK","C2-T8H",null,"Čelisti ke kleštím LK-2 na PC konektory stíněné RJ45-8p8c krátké Hirose","1pár",24.123124427075794,{"$f":"F4906*(1-Elteq!$F$9)","v":24.123124427075794},"8591735036034"]
["TECHNIK","C2-T8M5",null,"Čelisti ke kleštím LK-2 na PC konektory stíněné RJ45-8p8c Molex průměr 5mm","1pár",24.123124427075794,{"$f":"F4907*(1-Elteq!$F$9)","v":24.123124427075794},"8591735036041"]
["TECHNIK","C2-T8M6",null,"Čelisti ke kleštím LK-2 na PC konektory stíněné RJ45-8p8c AMP + Molex průměr 6mm","1pár",24.123124427075794,{"$f":"F4908*(1-Elteq!$F$9)","v":24.123124427075794},"8591735036058"]
["TECHNIK","C2-T8Q",null,"Čelisti ke kleštím LK-2 na PC konektory stíněné RJ45-8p8c dlouhé Hirose","1pár",24.123124427075794,{"$f":"F4909*(1-Elteq!$F$9)","v":24.123124427075794},"8591735035990"]
["TECHNIK","C2-T8S",null,"Čelisti ke kleštím LK-2 na PC konektory stíněné RJ45-8p8c krátké Stewart","1pár",23.009749453518449,{"$f":"F4910*(1-Elteq!$F$9)","v":23.009749453518449},"8591735023850"]
["TECHNIK","C2-X 1",null,"Čelisti ke kleštím LK-2 na koaxiální konektory RG 58, 59, 62","1pár",9.0925622840516453,{"$f":"F4911*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735008338"]
["TECHNIK","C2-X 2",null,"Čelisti ke kleštím LK-2 na koaxiální konektory RG 8, 11, 174, 179, 213","1pár",9.0925622840516453,{"$f":"F4912*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735008345"]
["TECHNIK","C2-X 3",null,"Čelisti ke kleštím LK-2 na koaxiální konektory RG 6, 58, 59, 62","1pár",9.0925622840516453,{"$f":"F4913*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735008352"]
["TECHNIK","C2-X 4",null,"Čelisti ke kleštím LK-2 na koaxiální konektory SMA, SMB, SMC, MCX","1pár",9.0925622840516453,{"$f":"F4914*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735010720"]
["TECHNIK","C2-X 5",null,"Čelisti ke kleštím LK-2 na koaxiální konektory RG 174, 179, Belden 8218 Fiber Optic","1pár",9.0925622840516453,{"$f":"F4915*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735010737"]
["TECHNIK","C2-X 6",null,"Čelisti ke kleštím LK-2 na koaxiální konektory CATV F RG 59, 6","1pár",9.0925622840516453,{"$f":"F4916*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735023874"]
["TECHNIK","C2-X 7",null,"Čelisti ke kleštím LK-2 na koaxiální konektory CATV F RG 59, 6","1pár",9.0925622840516453,{"$f":"F4917*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735023881"]
["TECHNIK","C2-X 8",null,"Čelisti ke kleštím LK-2 na koaxiální konektory RG 59, 6 (6,50/1,73/7,49mm)","1pár",9.0925622840516453,{"$f":"F4918*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735045296"]
["TECHNIK","C2-X 9",null,"Čelisti ke kleštím LK-2 na koaxiální konektory RG 58, 59, 6, 62, 142  (5,79/1,73/7,75mm)","1pár",9.0925622840516453,{"$f":"F4919*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735045302"]
["TECHNIK","CC-D 0510",null,"Čelisti ke kleštím LK-CC na dutinky pro průřezy 0,5-10mm2","1pár",28.947749312490952,{"$f":"F4920*(1-Elteq!$F$9)","v":28.947749312490952},"8591735035655"]
["TECHNIK","CC-D 1635",null,"Čelisti ke kleštím LK-CC na dutinky pro průřezy 16-35mm2","1pár",28.947749312490952,{"$f":"F4921*(1-Elteq!$F$9)","v":28.947749312490952},"8591735035662"]
["TECHNIK","CC-MO 056",null,"Čelisti ke kleštím LK-CC na mosazné objímky pro průřezy 0,5-6mm2","1pár",28.947749312490952,{"$f":"F4922*(1-Elteq!$F$9)","v":28.947749312490952},"8591735035679"]
["TECHNIK","CC-OI 056",null,"Čelisti ke kleštím LK-CC na oka, spojky a konektory s izolací 0,5-6mm2","1pár",28.947749312490952,{"$f":"F4923*(1-Elteq!$F$9)","v":28.947749312490952},"8591735035686"]
["TECHNIK","CC-ON 0510",null,"Čelisti ke kleštím LK-CC na oka a spojky bez izolace 0,5-10mm2","1pár",28.947749312490952,{"$f":"F4924*(1-Elteq!$F$9)","v":28.947749312490952},"8591735035693"]
["TECHNIK","CC-T6",null,"Čelisti ke kleštím LK-CC na PC konektory nestíněné RJ11-6p4c a RJ12-6p6c","1pár",28.947749312490952,{"$f":"F4925*(1-Elteq!$F$9)","v":28.947749312490952},"8591735035709"]
["TECHNIK","CC-T8C",null,"Čelisti ke kleštím LK-CC na PC konektory stíněné RJ45-8p8c Cimco","1pár",28.947749312490952,{"$f":"F4926*(1-Elteq!$F$9)","v":28.947749312490952},"8591735035716"]
["TECHNIK","CC-T8H",null,"Čelisti ke kleštím LK-CC na PC konektory stíněné RJ45-8p8c Hirose","1pár",28.947749312490952,{"$f":"F4927*(1-Elteq!$F$9)","v":28.947749312490952},"8591735035723"]
["TECHNIK","CC-T8S",null,"Čelisti ke kleštím LK-CC na PC konektory stíněné RJ45-8p8c Stewart Stamping","1pár",28.947749312490952,{"$f":"F4928*(1-Elteq!$F$9)","v":28.947749312490952},"8591735035730"]
["TECHNIK","CC-X 1",null,"Čelisti ke kleštím LK-CC na koaxiální konektory RG 58, 59, 62","1pár",28.947749312490952,{"$f":"F4929*(1-Elteq!$F$9)","v":28.947749312490952},"8591735035747"]
["TECHNIK","BF 190P",null,"Plyn Propan-Butan v propichovací kartuši 190g pro ST-MPH","1ks",1.8556249559289073,{"$f":"F4930*(1-Elteq!$F$9)","v":1.8556249559289073},""]
["TECHNIK","BF 55",null,"Plyn Butan v lahvi 156g pro plynové hořáky","1ks",5.7153248642610341,{"$f":"F4931*(1-Elteq!$F$9)","v":5.7153248642610341},""]
["TECHNIK","BZ 4500HS",null,"Plynový hořák s velkým plamenem na smršťování trubic spalující plyn Mapp a Propan","1ks",83.800023009749452,{"$f":"F4932*(1-Elteq!$F$9)","v":83.800023009749452},"8591735048679"]
["TECHNIK","JT 539T",null,"Plynový hořák pro letování natvrdo s TURBO plamenem spalující plyn MAPP a PROPAN","1ks",40.118611547182972,{"$f":"F4933*(1-Elteq!$F$9)","v":40.118611547182972},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"MG9",null,"Plyn MAPP v lahvi 400g pro plynové hořáky, max. teplota 2100 st.C / výkon 1478 W","1ks",16.21816211481865,{"$f":"F4934*(1-Elteq!$F$9)","v":16.21816211481865},""]
["TECHNIK","Pájka s Ag",null,"Bezolovnatá pájka průměr 1mm s tavidlem 2,5% složení Sn96,5 Ag3 Cu0,5 (500g)","1ks",51.58637377482362,{"$f":"F4935*(1-Elteq!$F$9)","v":51.58637377482362},"8591735037208"]
["TECHNIK","Pájka s Pb",null,"Olovnatá pájka průměr 1mm s tavidlem 2,5% složení Sn60 Pb40 (500g)","1ks",22.267499471146888,{"$f":"F4936*(1-Elteq!$F$9)","v":22.267499471146888},"8591735037215"]
["TECHNIK","PB175-E",null,"Plyn Propan-Butan v lahvi 175g (300ml)","1ks",7.0513748325298478,{"$f":"F4937*(1-Elteq!$F$9)","v":7.0513748325298478},""]
["TECHNIK","PB340-7/16",null,"Plyn Propan-Butan v lahvi 336g (600ml) se závitem 7/16\"","1ks",5.1957498766009405,{"$f":"F4938*(1-Elteq!$F$9)","v":5.1957498766009405},"8591735037277"]
["TECHNIK","PR 7/16",null,"Plynová redukce pro lahve se závitem 7/16\" k přístrojům Bernzomatic","1ks",17.257312090138839,{"$f":"F4939*(1-Elteq!$F$9)","v":17.257312090138839},"8591735037024"]
["TECHNIK","PS 135",null,"Plynový tužkový mikro hořák s jehlovým plamenem","1ks",85.17318547713684,{"$f":"F4940*(1-Elteq!$F$9)","v":85.17318547713684},"8591735053246"]
["TECHNIK","ST 1100 T",null,"Plynový mini hořák s letovacím bodovým hrotem","1ks",38.596999083321272,{"$f":"F4941*(1-Elteq!$F$9)","v":38.596999083321272},""]
["TECHNIK","ST 200 T",null,"Plynový tužkový mikro hořák s jehlovým plamenem (dříve ST100T)","1ks",22.267499471146888,{"$f":"F4942*(1-Elteq!$F$9)","v":22.267499471146888},"8591735046804"]
["TECHNIK","ST 2200 T",null,"Plynový mini hořák s letovacím bodovým hrotem (dříve ST1100T)","1ks",42.864936481957756,{"$f":"F4943*(1-Elteq!$F$9)","v":42.864936481957756},"8591735046811"]
["TECHNIK","ST 2200 T hrot",null,"Náhradní letovací bodový hrot k plynovému mini hořáku ST2200T","1ks",7.236937328122738,{"$f":"F4944*(1-Elteq!$F$9)","v":7.236937328122738},""]
["TECHNIK","ST 250 K",null,"Plynový tužkový mikro hořák s jehlovým plamenem v plastovém pouzdru (dříve ST150K)","1sada",30.692036771064128,{"$f":"F4945*(1-Elteq!$F$9)","v":30.692036771064128},"8591735046828"]
["TECHNIK","ST-HG 1",null,"Plynový mini hořák ke všeobecnému použití s přípravkem na smršťování bužírek","1ks",21.896374479961107,{"$f":"F4946*(1-Elteq!$F$9)","v":21.896374479961107},"8591735046835"]
["TECHNIK","ST-MPH",null,"Plynový multifunkční hořák s piezo-zapalováním (bez propichovací kartuše 190g propan-butan BF-190P)","1ks",24.791149411210203,{"$f":"F4947*(1-Elteq!$F$9)","v":24.791149411210203},"8591735046842"]
["TECHNIK","ST-RFR PIEZO",null,"Plynový hořák se závitem 7/16\" na propan-butan s lahví plynu 340g","1ks",68.658123369369576,{"$f":"F4948*(1-Elteq!$F$9)","v":68.658123369369576},"8591735046859"]
["TECHNIK","TS 3000T",null,"Plynový hořák Quickfire spalujíci plyn Propan v kartuši TX9","1ks",42.382473993416241,{"$f":"F4949*(1-Elteq!$F$9)","v":42.382473993416241},""]
["TECHNIK","TS 4000T",null,"Plynový hořák z kovové slitiny s tryskou spalující plyn MAPP a PROPAN","1ks",71.441560803262931,{"$f":"F4950*(1-Elteq!$F$9)","v":71.441560803262931},""]
["TECHNIK","TS 7000T",null,"Plynový hořák z kovové slitiny s TURBO tryskou spalující plyn MAPP a PROPAN","1ks",91.296747831702234,{"$f":"F4951*(1-Elteq!$F$9)","v":91.296747831702234},""]
["TECHNIK","TS 8000BT",null,"Plynový hořák z kovové slitiny s JUMBO tryskou spalující plyn MAPP a PROPAN","1ks",124.88355953401546,{"$f":"F4952*(1-Elteq!$F$9)","v":124.88355953401546},""]
["TECHNIK","TS 839T",null,"Plynový hořák s otočnou trubicí o 360° spalující plyn MAPP a PROPAN","1ks",49.582298822420405,{"$f":"F4953*(1-Elteq!$F$9)","v":49.582298822420405},""]
["TECHNIK","TX9",null,"Plyn Propan v lahvi 400g pro plynové hořáky, max. teplota 1870 st.C / výkon 870 W","1ks",10.577062248794771,{"$f":"F4954*(1-Elteq!$F$9)","v":10.577062248794771},""]
["TECHNIK","UL 100-E SET",null,"Mosazný hořák s tužkovým plamenem + Propan 400g","1sada",36.96404912210383,{"$f":"F4955*(1-Elteq!$F$9)","v":36.96404912210383},""]
["TECHNIK","VULCANE EXPRES",null,"Plynový hořák výkonný mobilní VULCANE EXPRESS s výměnnými tryskami spalující plyn MAPP a PROPAN","1ks",77.45378566047259,{"$f":"F4956*(1-Elteq!$F$9)","v":77.45378566047259},""]
["TECHNIK","KLS 0,14-1,5",null,"Lisovací kleště na rolované kontakty pro průřezy 0,14-1,5mm2, kvalitní Knipex","1ks",160.69712118344336,{"$f":"F4957*(1-Elteq!$F$9)","v":160.69712118344336},""]
["TECHNIK","KN 00 11 01",null,"001101 KNIPEX klíč na rozvodné skříně pro elektrikáře","1ks",28.279724328356547,{"$f":"F4958*(1-Elteq!$F$9)","v":28.279724328356547},""]
["TECHNIK","KN 00 11 02",null,"001102 KNIPEX klíč na rozvodné skříně pro elektrikáře","1ks",21.00567450111523,{"$f":"F4959*(1-Elteq!$F$9)","v":21.00567450111523},""]
["TECHNIK","KN 00 11 03",null,"001103 KNIPEX klíč na rozvodné skříně pro elektrikáře","1ks",21.228349495826699,{"$f":"F4960*(1-Elteq!$F$9)","v":21.228349495826699},""]
["TECHNIK","KN 00 20 17",null,"002017 KNIPEX sada kleští ESD pro elektroniku","1ks",253.25569398517726,{"$f":"F4961*(1-Elteq!$F$9)","v":253.25569398517726},""]
["TECHNIK","KN 00 21 01 TL",null,"002101TL KNIPEX 24-dílná brašna s nářadím do 1000V pro elektrikáře","1ks",420.29905251789751,{"$f":"F4962*(1-Elteq!$F$9)","v":420.29905251789751},""]
["TECHNIK","KN 00 21 02 LE",null,"002102LE KNIPEX brašna na nářadí prázdná","1ks",120.54139713714181,{"$f":"F4963*(1-Elteq!$F$9)","v":120.54139713714181},""]
["TECHNIK","KN 00 21 02 SL",null,"002102SL KNIPEX 24-dílná brašna s nářadím pro elektrikáře","1ks",348.74615421727884,{"$f":"F4964*(1-Elteq!$F$9)","v":348.74615421727884},""]
["TECHNIK","KN 00 21 05 LE",null,"002105LE KNIPEX kufr montážní prázdný typ BASIC","1ks",130.48754690092076,{"$f":"F4965*(1-Elteq!$F$9)","v":130.48754690092076},""]
["TECHNIK","KN 00 21 20 LE",null,"002120LE KNIPEX kufr montážní prázdný","1ks",218.85240730225533,{"$f":"F4966*(1-Elteq!$F$9)","v":218.85240730225533},""]
["TECHNIK","KN 00 21 40 LE",null,"002140LE KNIPEX kufr montážní prázdný","1ks",311.33675510575205,{"$f":"F4967*(1-Elteq!$F$9)","v":311.33675510575205},""]
["TECHNIK","KN 00 21 41 LE",null,"002141LE KNIPEX kufr montážní prázdný","1ks",362.70045388586419,{"$f":"F4968*(1-Elteq!$F$9)","v":362.70045388586419},"8591735047146"]
["TECHNIK","KN 02 01 180",null,"0201180 KNIPEX kleště kombinované silné, rukojeti potažené PVC, délka 180mm","1ks",17.479987084850308,{"$f":"F4969*(1-Elteq!$F$9)","v":17.479987084850308},""]
["TECHNIK","KN 02 01 200",null,"0201200 KNIPEX kleště kombinované silné, rukojeti potažené PVC, délka 200mm","1ks",18.444912061933337,{"$f":"F4970*(1-Elteq!$F$9)","v":18.444912061933337},""]
["TECHNIK","KN 02 02 180",null,"0202180 KNIPEX kleště kombinované silné, dvoukomponentní rukojeti, délka 180mm","1ks",19.780962030202151,{"$f":"F4971*(1-Elteq!$F$9)","v":19.780962030202151},""]
["TECHNIK","KN 02 02 200",null,"0202200 KNIPEX kleště kombinované silné, dvoukomponentní rukojeti, délka 200mm","1ks",21.488136989656745,{"$f":"F4972*(1-Elteq!$F$9)","v":21.488136989656745},""]
["TECHNIK","KN 02 06 180",null,"0206180 KNIPEX kleště kombinované silné do 1000V, chromované, dvoukomponentní rukojeti, délka 180mm","1ks",28.057049333645079,{"$f":"F4973*(1-Elteq!$F$9)","v":28.057049333645079},""]
["TECHNIK","KN 02 06 200",null,"0206200 KNIPEX kleště kombinované silné do 1000V, chromované, dvoukomponentní rukojeti, délka 200mm","1ks",29.578661797506783,{"$f":"F4974*(1-Elteq!$F$9)","v":29.578661797506783},""]
["TECHNIK","KN 03 01 160",null,"0301160 KNIPEX kleště kombinované, rukojeti potažené PVC, délka 160mm","1ks",12.098674712656475,{"$f":"F4975*(1-Elteq!$F$9)","v":12.098674712656475},""]
["TECHNIK","KN 03 01 180",null,"0301180 KNIPEX kleště kombinované, rukojeti potažené PVC, délka 180mm","1ks",12.952262192383772,{"$f":"F4976*(1-Elteq!$F$9)","v":12.952262192383772},""]
["TECHNIK","KN 03 01 200",null,"0301200 KNIPEX kleště kombinované, rukojeti potažené PVC, délka 200mm","1ks",14.956337144786993,{"$f":"F4977*(1-Elteq!$F$9)","v":14.956337144786993},""]
["TECHNIK","KN 03 02 160",null,"0302160 KNIPEX kleště kombinované, dvoukomponentní rukojeti, délka 160mm","1ks",15.735699626277134,{"$f":"F4978*(1-Elteq!$F$9)","v":15.735699626277134},""]
["TECHNIK","KN 03 02 180",null,"0302180 KNIPEX kleště kombinované, dvoukomponentní rukojeti, délka 180mm","1ks",15.99548712010718,{"$f":"F4979*(1-Elteq!$F$9)","v":15.99548712010718},""]
["TECHNIK","KN 03 02 200",null,"0302200 KNIPEX kleště kombinované, dvoukomponentní rukojeti, délka 200mm","1ks",18.444912061933337,{"$f":"F4980*(1-Elteq!$F$9)","v":18.444912061933337},""]
["TECHNIK","KN 03 06 160",null,"0306160 KNIPEX kleště kombinované do 1000V, chromované, dvoukomponentní rukojeti, délka 160mm","1ks",21.859261980842529,{"$f":"F4981*(1-Elteq!$F$9)","v":21.859261980842529},""]
["TECHNIK","KN 03 06 180",null,"0306180 KNIPEX kleště kombinované do 1000V, chromované, dvoukomponentní rukojeti, délka 180mm","1ks",23.529324441178545,{"$f":"F4982*(1-Elteq!$F$9)","v":23.529324441178545},""]
["TECHNIK","KN 03 06 200",null,"0306200 KNIPEX kleště kombinované do 1000V, chromované, dvoukomponentní rukojeti, délka 200mm","1ks",26.312761875071907,{"$f":"F4983*(1-Elteq!$F$9)","v":26.312761875071907},""]
["TECHNIK","KN 08 05 110",null,"0805110 KNIPEX kleště kombinované pro mikroelektroniku, délka 110mm","1ks",22.267499471146888,{"$f":"F4984*(1-Elteq!$F$9)","v":22.267499471146888},""]
["TECHNIK","KN 11 01 160",null,"1101160 KNIPEX kleště odizolovací, rukojeti potažené PVC, délka 160mm","1ks",17.071749594545945,{"$f":"F4985*(1-Elteq!$F$9)","v":17.071749594545945},""]
["TECHNIK","KN 11 02 160",null,"1102160 KNIPEX kleště odizolovací, dvoukomponentní rukojeti, délka 160mm","1ks",20.63454950992945,{"$f":"F4986*(1-Elteq!$F$9)","v":20.63454950992945},""]
["TECHNIK","KN 11 06 160",null,"1106160 KNIPEX kleště odizolovací do 1000V, chromované, dvoukomponentní rukojeti, délka 160mm","1ks",27.277686852154936,{"$f":"F4987*(1-Elteq!$F$9)","v":27.277686852154936},""]
["TECHNIK","KN 11 92 140",null,"1192140 KNIPEX kleště odizolovací pro mikroelektroniku, délka 140mm","1ks",45.462811420258227,{"$f":"F4988*(1-Elteq!$F$9)","v":45.462811420258227},""]
["TECHNIK","KN 12 62 180",null,"1262180 KNIPEX kleště odizolovací automatické 0,2-6,0mm2, délka 180mm (Jokari)","1ks",34.106386689973313,{"$f":"F4989*(1-Elteq!$F$9)","v":34.106386689973313},""]
["TECHNIK","KN 12 80 100 SB",null,"1280100 KNIPEX miniodizolovací nůž pro průměry vodičů 0,25-0,8mm, délka 100mm","1ks",42.271136496060507,{"$f":"F4990*(1-Elteq!$F$9)","v":42.271136496060507},""]
["TECHNIK","KN 13 01 160",null,"1301160 KNIPEX kleště drátovací, rukojeti potažené PVC, délka 160mm","1ks",30.246686781641188,{"$f":"F4991*(1-Elteq!$F$9)","v":30.246686781641188},""]
["TECHNIK","KN 13 02 160",null,"1302160 KNIPEX kleště drátovací, dvoukomponentní rukojeti, délka 160mm","1ks",31.99097424021436,{"$f":"F4992*(1-Elteq!$F$9)","v":31.99097424021436},""]
["TECHNIK","KN 13 05 160",null,"1305160 KNIPEX kleště drátovací chromované, dvoukomponentní rukojeti, délka 160mm","1ks",36.518699132680894,{"$f":"F4993*(1-Elteq!$F$9)","v":36.518699132680894},""]
["TECHNIK","KN 13 81 200",null,"1381200 KNIPEX kleště kombinované elektro potažené PVC, délka 200mm","1ks",42.085574000467616,{"$f":"F4994*(1-Elteq!$F$9)","v":42.085574000467616},""]
["TECHNIK","KN 13 96 200",null,"1396200 KNIPEX kleště kombinované elektro, dvoukomponentní rukojeti do 1000V, délka 200mm","1ks",50.992573788926371,{"$f":"F4995*(1-Elteq!$F$9)","v":50.992573788926371},""]
["TECHNIK","KN 14 22 160",null,"1422160 KNIPEX kleště stranové štípací / odizolovací, délka 160","1ks",32.696111723467347,{"$f":"F4996*(1-Elteq!$F$9)","v":32.696111723467347},""]
["TECHNIK","KN 14 26 160",null,"1426160 KNIPEX kleště stranové štípací / odizolovací do 1000V, délka 160mm","1ks",39.227911568337099,{"$f":"F4997*(1-Elteq!$F$9)","v":39.227911568337099},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"KN 16 20 165 SB",null,"1620165 KNIPEX nůž odplášťovací s hákem na kabely o průměru 8-28mm","1ks",21.302574494063855,{"$f":"F4998*(1-Elteq!$F$9)","v":21.302574494063855},""]
["TECHNIK","KN 16 29 165",null,"1629165 KNIPEX náhradní břit k odplášťovacímu noži, 2ks v sadě","2ks",6.420462347514019,{"$f":"F4999*(1-Elteq!$F$9)","v":6.420462347514019},""]
["TECHNIK","KN 16 60 05 SB",null,"166005 KNIPEX nůž odplášťovací na koaxiální kabely RG 58, RG 59 a RG 62","1ks",21.154124497589542,{"$f":"F5000*(1-Elteq!$F$9)","v":21.154124497589542},""]
["TECHNIK","KN 16 60 100 SB",null,"1660100 KNIPEX nůž odplášťovací na koaxiální kabely o průměru 4,8-7,5mm","1ks",21.636586986131061,{"$f":"F5001*(1-Elteq!$F$9)","v":21.636586986131061},""]
["TECHNIK","KN 16 65 125 SB",null,"1665125 KNIPEX nůž odplášťovací na datové kabely CAT 5, CAT 6, CAT 7 kroucené páry (UTP/STP)","1ks",40.452624039250182,{"$f":"F5002*(1-Elteq!$F$9)","v":40.452624039250182},""]
["TECHNIK","KN 16 80 125 SB",null,"1680125 KNIPEX nůž odplášťovací na kabely o průměru 8-13mm nebo průřezu 3x1,5mm2 až 5x2,5mm2","1ks",21.970599478198263,{"$f":"F5003*(1-Elteq!$F$9)","v":21.970599478198263},""]
["TECHNIK","KN 16 85 125 SB",null,"1685125 KNIPEX nůž odplášťovací na kabely o průměru 8-13mm nebo průřezu 3x1,5mm2 až 5x2,5mm2","1ks",39.561924060404301,{"$f":"F5004*(1-Elteq!$F$9)","v":39.561924060404301},""]
["TECHNIK","KN 19 01 130",null,"1901130 KNIPEX kleště očkové kulaté jemné se štípáním, délka 130mm","1ks",24.976711906803093,{"$f":"F5005*(1-Elteq!$F$9)","v":24.976711906803093},""]
["TECHNIK","KN 19 03 130",null,"1903130 KNIPEX kleště očkové kulaté jemné se štípáním, chromované, délka 130mm","1ks",28.428174324830859,{"$f":"F5006*(1-Elteq!$F$9)","v":28.428174324830859},""]
["TECHNIK","KN 20 02 160",null,"2002160 KNIPEX kleště ploché, dvoukomponentní rukojeti, délka 160mm","1ks",15.624362128921399,{"$f":"F5007*(1-Elteq!$F$9)","v":15.624362128921399},""]
["TECHNIK","KN 22 01 160",null,"2201160 KNIPEX kleště očkové kulaté, rukojeti potažené PVC, délka 160mm","1ks",13.323387183569555,{"$f":"F5008*(1-Elteq!$F$9)","v":13.323387183569555},""]
["TECHNIK","KN 22 01 180",null,"2201180 KNIPEX kleště očkové kulaté, rukojeti potažené PVC, délka 180mm","1ks",15.550137130684243,{"$f":"F5009*(1-Elteq!$F$9)","v":15.550137130684243},""]
["TECHNIK","KN 22 02 160",null,"2202160 KNIPEX kleště očkové kulaté, dvoukomponentní rukojeti, délka 160mm","1ks",15.475912132447087,{"$f":"F5010*(1-Elteq!$F$9)","v":15.475912132447087},""]
["TECHNIK","KN 22 06 160",null,"2206160 KNIPEX kleště očkové kulaté do 1000V, dvoukomponentní rukojeti, délka 160mm","1ks",22.341724469384044,{"$f":"F5011*(1-Elteq!$F$9)","v":22.341724469384044},""]
["TECHNIK","KN 22 07 160",null,"2207160 KNIPEX kleště očkové kulaté do 1000V, izolované rukojeti, délka 160mm","1ks",27.20346185391778,{"$f":"F5012*(1-Elteq!$F$9)","v":27.20346185391778},""]
["TECHNIK","KN 23 01 140",null,"2301140 KNIPEX kleště ploché, rukojeti potažené PVC, délka 140mm","1ks",21.079899499352386,{"$f":"F5013*(1-Elteq!$F$9)","v":21.079899499352386},""]
["TECHNIK","KN 25 01 160",null,"2501160 KNIPEX kleště půlkulaté, rukojeti potažené PVC, délka 160mm","1ks",15.80992462451429,{"$f":"F5014*(1-Elteq!$F$9)","v":15.80992462451429},""]
["TECHNIK","KN 25 02 140",null,"2502140 KNIPEX kleště půlkulaté s břity, dvoukomponentní rukojeti, délka 140mm","1ks",18.185124568103291,{"$f":"F5015*(1-Elteq!$F$9)","v":18.185124568103291},""]
["TECHNIK","KN 25 02 160",null,"2502160 KNIPEX kleště půlkulaté s břity, dvoukomponentní rukojeti, délka 160mm","1ks",18.482024561051915,{"$f":"F5016*(1-Elteq!$F$9)","v":18.482024561051915},""]
["TECHNIK","KN 25 06 160",null,"2506160 KNIPEX kleště půlkulaté s břity do 1000V, chromované, dvoukomponentní rukojeti, délka 160mm","1ks",24.345799421787262,{"$f":"F5017*(1-Elteq!$F$9)","v":24.345799421787262},""]
["TECHNIK","KN 25 25 160",null,"2525160 KNIPEX kleště půlkulaté s břity, chromované, dvoukomponentní rukojeti, délka 160mm","1ks",24.791149411210203,{"$f":"F5018*(1-Elteq!$F$9)","v":24.791149411210203},""]
["TECHNIK","KN 25 26 160",null,"2526160 KNIPEX kleště půlkulaté s břity do 1000V, chromované, dvoukomponentní rukojeti, délka 160mm","1ks",27.351911850392092,{"$f":"F5019*(1-Elteq!$F$9)","v":27.351911850392092},""]
["TECHNIK","KN 26 11 200",null,"2611200 KNIPEX kleště půlkulaté dlouhé se štípáním, rukojeti potažené PVC, délka 200mm","1ks",20.448987014336559,{"$f":"F5020*(1-Elteq!$F$9)","v":20.448987014336559},""]
["TECHNIK","KN 26 12 200",null,"2612200 KNIPEX kleště půlkulaté dlouhé se štípáním, dvoukomponentní rukojeti, délka 200mm","1ks",22.935524455281293,{"$f":"F5021*(1-Elteq!$F$9)","v":22.935524455281293},""]
["TECHNIK","KN 26 16 200",null,"2616200 KNIPEX kleště půlkulaté dlouhé do 1000V, chromované, dvoukomponentní rukojeti, délka 200mm","1ks",29.875561790455407,{"$f":"F5022*(1-Elteq!$F$9)","v":29.875561790455407},""]
["TECHNIK","KN 26 21 200",null,"2621200 KNIPEX kleště půlkulaté dlouhé zahnuté se štípáním, rukojeti potažené PVC, délka 200mm","1ks",23.121086950874187,{"$f":"F5023*(1-Elteq!$F$9)","v":23.121086950874187},""]
["TECHNIK","KN 26 22 200",null,"2622200 KNIPEX kleště půlkulaté dlouhé zahnuté se štípáním, dvoukomponentní rukojeti, délka 200mm","1ks",25.384949397107452,{"$f":"F5024*(1-Elteq!$F$9)","v":25.384949397107452},"8591735013332"]
["TECHNIK","KN 26 26 200",null,"2626200 KNIPEX kleště půlkulaté dlouhé zahnuté do 1000V, chromované, dvoukomponentní rukojeti","1ks",33.549699203194642,{"$f":"F5025*(1-Elteq!$F$9)","v":33.549699203194642},""]
["TECHNIK","KN 26 27 200",null,"2627200 KNIPEX kleště půlkulaté dlouhé zahnuté do 1000V, chromované, masivní rukojeti","1ks",39.302136566574255,{"$f":"F5026*(1-Elteq!$F$9)","v":39.302136566574255},""]
["TECHNIK","KN 29 25 160",null,"2925160 KNIPEX kleště půlkulaté telefonní, chromované, dvoukomponentní rukojeti, délka 160mm","1ks",24.902486908565937,{"$f":"F5027*(1-Elteq!$F$9)","v":24.902486908565937},""]
["TECHNIK","KN 30 11 160",null,"3011160 KNIPEX kleště ploché, rukojeti potažené PVC, délka 160mm","1ks",16.106824617462916,{"$f":"F5028*(1-Elteq!$F$9)","v":16.106824617462916},""]
["TECHNIK","KN 30 11 190",null,"3011190 KNIPEX kleště ploché, rukojeti potažené PVC, délka 190mm","1ks",18.519137060170493,{"$f":"F5029*(1-Elteq!$F$9)","v":18.519137060170493},""]
["TECHNIK","KN 30 15 160",null,"3015160 KNIPEX kleště ploché, chromované, dvoukomponentní rukojeti, délka 160mm","1ks",22.824186957925559,{"$f":"F5030*(1-Elteq!$F$9)","v":22.824186957925559},""]
["TECHNIK","KN 30 15 190",null,"3015190 KNIPEX kleště ploché, chromované, dvoukomponentní rukojeti, délka 190mm","1ks",25.125161903277405,{"$f":"F5031*(1-Elteq!$F$9)","v":25.125161903277405},""]
["TECHNIK","KN 30 16 160",null,"3016160 KNIPEX kleště ploché do 1000V, chromované, dvoukomponentní rukojeti, délka 160mm","1ks",25.125161903277405,{"$f":"F5032*(1-Elteq!$F$9)","v":25.125161903277405},""]
["TECHNIK","KN 30 25 140",null,"3025140 KNIPEX kleště půlkulaté, chromované, dvoukomponentní rukojeti, délka 140mm","1ks",21.859261980842529,{"$f":"F5033*(1-Elteq!$F$9)","v":21.859261980842529},""]
["TECHNIK","KN 30 31 160",null,"3031160 KNIPEX kleště zakulacené dlouhé, rukojeti potažené PVC, délka 160mm","1ks",15.99548712010718,{"$f":"F5034*(1-Elteq!$F$9)","v":15.99548712010718},""]
["TECHNIK","KN 30 35 160",null,"3035160 KNIPEX kleště zakulacené dlouhé, dvoukomponentní rukojeti, délka 160mm","1ks",21.859261980842529,{"$f":"F5035*(1-Elteq!$F$9)","v":21.859261980842529},""]
["TECHNIK","KN 30 36 160",null,"3036160 KNIPEX kleště zakulacené dlouhé do 1000V, dvoukomponentní rukojeti, délka 160mm","1ks",24.902486908565937,{"$f":"F5036*(1-Elteq!$F$9)","v":24.902486908565937},""]
["TECHNIK","KN 31 11 160",null,"3111160 KNIPEX kleště půlkulaté rovné jemné, rukojeti potažené PVC, délka 160mm","1ks",24.160236926194372,{"$f":"F5037*(1-Elteq!$F$9)","v":24.160236926194372},""]
["TECHNIK","KN 31 25 160",null,"3125160 KNIPEX kleště půlkulaté zahnuté jemné, chromované, dvoukomponentní rukojeti, délka 160mm","1ks",33.438361705838908,{"$f":"F5038*(1-Elteq!$F$9)","v":33.438361705838908},""]
["TECHNIK","KN 33 01 160",null,"3301160 KNIPEX kleště ploché speciální, rukojeti potažené PVC, délka 160mm","1ks",25.79318688741181,{"$f":"F5039*(1-Elteq!$F$9)","v":25.79318688741181},""]
["TECHNIK","KN 35 12 115",null,"3512115 KNIPEX kleště ploché leštěné pro mikroelektroniku, dvoukomponentní rukojeti, délka 115mm","1ks",28.539511822186594,{"$f":"F5040*(1-Elteq!$F$9)","v":28.539511822186594},""]
["TECHNIK","KN 35 22 115",null,"3522115 KNIPEX kleště půlkulaté pro elektroniku, leštěné, dvoukomponentní rukojeti, délka 115mm","1ks",28.539511822186594,{"$f":"F5041*(1-Elteq!$F$9)","v":28.539511822186594},""]
["TECHNIK","KN 35 32 115",null,"3532115 KNIPEX kleště kulaté pro elektroniku, leštěné, dvoukomponentní rukojeti, délka 115mm","1ks",28.539511822186594,{"$f":"F5042*(1-Elteq!$F$9)","v":28.539511822186594},""]
["TECHNIK","KN 35 42 115",null,"3542115 KNIPEX kleště půlkulaté zahnuté pro elektroniku, leštěné, dvoukomponentní rukojeti","1ks",30.803374268419862,{"$f":"F5043*(1-Elteq!$F$9)","v":30.803374268419862},""]
["TECHNIK","KN 35 62 145",null,"3562145 KNIPEX kleště půlkulaté pro elektroniku, leštěné, dvoukomponentní rukojeti, délka 145mm","1ks",32.25076173404441,{"$f":"F5044*(1-Elteq!$F$9)","v":32.25076173404441},""]
["TECHNIK","KN 38 15 200",null,"3815200 KNIPEX kleště půlkulaté dlouhé rovné, dvoukomponentní rukojeti, délka 200mm","1ks",28.762186816898062,{"$f":"F5045*(1-Elteq!$F$9)","v":28.762186816898062},""]
["TECHNIK","KN 38 71 200",null,"3871200 KNIPEX kleště půlkulaté dlouhé zahnuté, rukojeti potažené PVC, délka 200mm","1ks",26.758111864494843,{"$f":"F5046*(1-Elteq!$F$9)","v":26.758111864494843},""]
["TECHNIK","KN 40 04 180",null,"4004180 KNIPEX kleště univerzální samosvorné s pákovým mechanismem, délka 180mm","1ks",20.374762016099403,{"$f":"F5047*(1-Elteq!$F$9)","v":20.374762016099403},""]
["TECHNIK","KN 44 11 J0",null,"4411J0 KNIPEX kleště SEEGER přímé 8-13mm vnitřní","1ks",12.210012210012209,{"$f":"F5048*(1-Elteq!$F$9)","v":12.210012210012209},""]
["TECHNIK","KN 44 11 J1",null,"4411J1 KNIPEX kleště SEEGER přímé 12-25mm vnitřní","1ks",12.210012210012209,{"$f":"F5049*(1-Elteq!$F$9)","v":12.210012210012209},""]
["TECHNIK","KN 44 11 J2",null,"4411J2 KNIPEX kleště SEEGER přímé 19-60mm vnitřní","1ks",13.063599689739508,{"$f":"F5050*(1-Elteq!$F$9)","v":13.063599689739508},""]
["TECHNIK","KN 44 11 J3",null,"4411J3 KNIPEX kleště SEEGER přímé 40-100mm vnitřní","1ks",14.80788714831268,{"$f":"F5051*(1-Elteq!$F$9)","v":14.80788714831268},""]
["TECHNIK","KN 44 11 J4",null,"4411J4 KNIPEX kleště SEEGER přímé 85-140mm vnitřní","1ks",25.013824405921671,{"$f":"F5052*(1-Elteq!$F$9)","v":25.013824405921671},""]
["TECHNIK","KN 44 21 J01",null,"4421J01 KNIPEX kleště SEEGER zahnuté 8-15mm vnitřní","1ks",13.917187169466805,{"$f":"F5053*(1-Elteq!$F$9)","v":13.917187169466805},""]
["TECHNIK","KN 44 21 J11",null,"4421J11 KNIPEX kleště SEEGER zahnuté 12-25mm vnitřní","1ks",13.917187169466805,{"$f":"F5054*(1-Elteq!$F$9)","v":13.917187169466805},""]
["TECHNIK","KN 44 21 J21",null,"4421J21 KNIPEX kleště SEEGER zahnuté 19-60mm vnitřní","1ks",14.176974663296852,{"$f":"F5055*(1-Elteq!$F$9)","v":14.176974663296852},""]
["TECHNIK","KN 44 21 J31",null,"4421J31 KNIPEX kleště SEEGER zahnuté 40-100mm vnitřní","1ks",15.698587127158556,{"$f":"F5056*(1-Elteq!$F$9)","v":15.698587127158556},""]
["TECHNIK","KN 44 21 J41",null,"4421J41 KNIPEX kleště SEEGER zahnuté 85-200mm vnitřní","1ks",26.758111864494843,{"$f":"F5057*(1-Elteq!$F$9)","v":26.758111864494843},""]
["TECHNIK","KN 46 11 A0",null,"4611A0 KNIPEX kleště SEEGER přímé 3-10mm vnější","1ks",14.176974663296852,{"$f":"F5058*(1-Elteq!$F$9)","v":14.176974663296852},""]
["TECHNIK","KN 46 11 A1",null,"4611A1 KNIPEX kleště SEEGER přímé 10-25mm vnější","1ks",13.471837180043867,{"$f":"F5059*(1-Elteq!$F$9)","v":13.471837180043867},""]
["TECHNIK","KN 46 11 A2",null,"4611A2 KNIPEX klleště SEEGER přímé 19-60mm vnější","1ks",14.80788714831268,{"$f":"F5060*(1-Elteq!$F$9)","v":14.80788714831268},""]
["TECHNIK","KN 46 11 A3",null,"4611A3 KNIPEX kleště SEEGER přímé 40-100mm vnější","1ks",16.069712118344338,{"$f":"F5061*(1-Elteq!$F$9)","v":16.069712118344338},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"KN 46 11 A4",null,"4611A4 KNIPEX kleště SEEGER přímé 85-165mm vnější","1ks",28.057049333645079,{"$f":"F5062*(1-Elteq!$F$9)","v":28.057049333645079},""]
["TECHNIK","KN 46 21 A01",null,"4621A01 KNIPEX kleště SEEGER zahnuté 3-10mm vnější","1ks",15.475912132447087,{"$f":"F5063*(1-Elteq!$F$9)","v":15.475912132447087},""]
["TECHNIK","KN 46 21 A11",null,"4621A11 KNIPEX kleště SEEGER zahnuté 10-25mm vnější","1ks",14.659437151838368,{"$f":"F5064*(1-Elteq!$F$9)","v":14.659437151838368},""]
["TECHNIK","KN 46 21 A21",null,"4621A21 KNIPEX kleště SEEGER zahnuté 19-60mm vnější","1ks",16.069712118344338,{"$f":"F5065*(1-Elteq!$F$9)","v":16.069712118344338},""]
["TECHNIK","KN 46 21 A31",null,"4621A31 KNIPEX kleště SEEGER zahnuté 40-100mm vnější","1ks",17.81399957691751,{"$f":"F5066*(1-Elteq!$F$9)","v":17.81399957691751},""]
["TECHNIK","KN 46 21 A41",null,"4621A41 KNIPEX kleště SEEGER zahnuté 85-145mm vnější","1ks",30.432249277234078,{"$f":"F5067*(1-Elteq!$F$9)","v":30.432249277234078},""]
["TECHNIK","KN 50 01 180",null,"5001180 KNIPEX kleště štípací, rukojeti potažené PVC, délka 180mm","1ks",13.620287176518179,{"$f":"F5068*(1-Elteq!$F$9)","v":13.620287176518179},""]
["TECHNIK","KN 50 01 210",null,"5001210 KNIPEX kleště štípací, rukojeti potažené PVC, délka 210mm","1ks",14.176974663296852,{"$f":"F5069*(1-Elteq!$F$9)","v":14.176974663296852},""]
["TECHNIK","KN 50 01 225",null,"5001225 KNIPEX kleště štípací, rukojeti potažené PVC, délka 225mm","1ks",16.21816211481865,{"$f":"F5070*(1-Elteq!$F$9)","v":16.21816211481865},""]
["TECHNIK","KN 50 01 250",null,"5001250 KNIPEX kleště štípací, rukojeti potažené PVC, délka 250mm","1ks",19.632512033727838,{"$f":"F5071*(1-Elteq!$F$9)","v":19.632512033727838},""]
["TECHNIK","KN 51 01 210",null,"5101210 KNIPEX kleště štípací s kladivem, rukojeti potažené PVC, délka 210mm","1ks",17.071749594545945,{"$f":"F5072*(1-Elteq!$F$9)","v":17.071749594545945},""]
["TECHNIK","KN 61 01 200",null,"6101200 KNIPEX kleště štípací čelní, rukojeti potažené PVC, délka 200mm","1ks",45.128798928191024,{"$f":"F5073*(1-Elteq!$F$9)","v":45.128798928191024},""]
["TECHNIK","KN 62 12 120",null,"6212120 KNIPEX kleště štípací pro elektroniku, dvoukomponentní rukojeti, délka 120mm","1ks",33.698149199668954,{"$f":"F5074*(1-Elteq!$F$9)","v":33.698149199668954},""]
["TECHNIK","KN 64 11 115",null,"6411115 KNIPEX kleště štípací pro elektroniku, dvoukomponentní rukojeti, délka 115mm","1ks",32.06519923845152,{"$f":"F5075*(1-Elteq!$F$9)","v":32.06519923845152},""]
["TECHNIK","KN 64 12 115 ESD",null,"6412115ESD KNIPEX kleště štípací pro elektroniku, antistatické provedení, délka 115mm","1ks",41.194874021621743,{"$f":"F5076*(1-Elteq!$F$9)","v":41.194874021621743},""]
["TECHNIK","KN 64 32 120",null,"6432120 KNIPEX kleště štípací pro elektroniku, dvoukomponentní rukojeti, délka 120mm","1ks",42.271136496060507,{"$f":"F5077*(1-Elteq!$F$9)","v":42.271136496060507},""]
["TECHNIK","KN 64 52 115",null,"6452115 KNIPEX kleště štípací pro elektroniku, dvoukomponentní rukojeti, délka 115mm","1ks",42.864936481957756,{"$f":"F5078*(1-Elteq!$F$9)","v":42.864936481957756},""]
["TECHNIK","KN 64 62 120",null,"6462120 KNIPEX kleště štípací pro elektroniku, dvoukomponentní rukojeti, délka 120mm","1ks",43.384511469617856,{"$f":"F5079*(1-Elteq!$F$9)","v":43.384511469617856},""]
["TECHNIK","KN 67 01 200",null,"6701200 KNIPEX kleště štípací čelní silné, rukojeti potažené PVC, délka 200mm","1ks",31.916749241977204,{"$f":"F5080*(1-Elteq!$F$9)","v":31.916749241977204},""]
["TECHNIK","KN 67 05 200",null,"6705200 KNIPEX kleště štípací čelní silné, dvoukomponentní rukojeti, délka 200mm","1ks",40.823749030435962,{"$f":"F5081*(1-Elteq!$F$9)","v":40.823749030435962},""]
["TECHNIK","KN 70 01 140",null,"7001140 KNIPEX kleště štípací stranové, rukojeti potažené PVC, délka 140mm","1ks",15.587249629802821,{"$f":"F5082*(1-Elteq!$F$9)","v":15.587249629802821},""]
["TECHNIK","KN 70 01 160",null,"7001160 KNIPEX kleště štípací stranové, rukojeti potažené PVC, délka 160mm","1ks",15.847037123632868,{"$f":"F5083*(1-Elteq!$F$9)","v":15.847037123632868},""]
["TECHNIK","KN 70 01 180",null,"7001180 KNIPEX kleště štípací stranové, rukojeti potažené PVC, délka 180mm","1ks",17.331537088375995,{"$f":"F5084*(1-Elteq!$F$9)","v":17.331537088375995},""]
["TECHNIK","KN 70 02 140",null,"7002140 KNIPEX kleště štípací stranové, dvoukomponentní rukojeti, délka 140mm","1ks",19.261387042542058,{"$f":"F5085*(1-Elteq!$F$9)","v":19.261387042542058},""]
["TECHNIK","KN 70 02 160",null,"7002160 KNIPEX kleště štípací stranové, dvoukomponentní rukojeti, délka 160mm","1ks",19.780962030202151,{"$f":"F5086*(1-Elteq!$F$9)","v":19.780962030202151},""]
["TECHNIK","KN 70 02 180",null,"7002180 KNIPEX kleště štípací stranové, dvoukomponentní rukojeti, délka 180mm","1ks",21.228349495826699,{"$f":"F5087*(1-Elteq!$F$9)","v":21.228349495826699},""]
["TECHNIK","KN 70 05 160",null,"7005160 KNIPEX kleště štípací stranové, chromované, dvoukomponentní rukojeti, délka 160mm","1ks",23.529324441178545,{"$f":"F5088*(1-Elteq!$F$9)","v":23.529324441178545},""]
["TECHNIK","KN 70 06 140",null,"7006140 KNIPEX kleště štípací stranové do 1000V, dvoukomponentní rukojeti, délka 140mm","1ks",24.976711906803093,{"$f":"F5089*(1-Elteq!$F$9)","v":24.976711906803093},""]
["TECHNIK","KN 70 06 160",null,"7006160 KNIPEX kleště štípací stranové do 1000V, dvoukomponentní rukojeti, délka 160mm","1ks",26.795224363613421,{"$f":"F5090*(1-Elteq!$F$9)","v":26.795224363613421},""]
["TECHNIK","KN 70 06 180",null,"7006180 KNIPEX kleště štípací stranové do 1000V, dvoukomponentní rukojeti, délka 180mm","1ks",28.79929931601664,{"$f":"F5091*(1-Elteq!$F$9)","v":28.79929931601664},""]
["TECHNIK","KN 70 07 160",null,"7007160 KNIPEX kleště štípací stranové do 1000V, izolované rukojeti, délka 160mm","1ks",31.322949256079955,{"$f":"F5092*(1-Elteq!$F$9)","v":31.322949256079955},""]
["TECHNIK","KN 70 07 180",null,"7007180 KNIPEX kleště štípací stranové do 1000V, izolované rukojeti, délka 180mm","1ks",33.809486697024688,{"$f":"F5093*(1-Elteq!$F$9)","v":33.809486697024688},""]
["TECHNIK","KN 70 11 110",null,"7011110 KNIPEX kleště štípací stranové, rukojeti potažené PVC, délka 110mm","1ks",20.337649516980825,{"$f":"F5094*(1-Elteq!$F$9)","v":20.337649516980825},""]
["TECHNIK","KN 70 26 160",null,"7026160 KNIPEX kleště štípací stranové do 1000V, dvoukomponentní rukojeti, délka 160mm","1ks",26.906561860969155,{"$f":"F5095*(1-Elteq!$F$9)","v":26.906561860969155},""]
["TECHNIK","KN 71 02 200",null,"7102200 KNIPEX nůžky pákové jednoruční na Fe dráty do průměru 4-6mm, masivní rukojeti","1ks",37.372286612408196,{"$f":"F5096*(1-Elteq!$F$9)","v":37.372286612408196},""]
["TECHNIK","KN 71 41 200",null,"7141200 KNIPEX nůžky pákové jednoruční na Fe dráty do průměru 4-6mm, vyhnuté","1ks",45.462811420258227,{"$f":"F5097*(1-Elteq!$F$9)","v":45.462811420258227},""]
["TECHNIK","KN 72 01 140",null,"7201140 KNIPEX kleště štípací stranové na plasty bez fazety, délka 140mm","1ks",21.488136989656745,{"$f":"F5098*(1-Elteq!$F$9)","v":21.488136989656745},""]
["TECHNIK","KN 72 01 160",null,"7201160 KNIPEX kleště štípací stranové na plasty bez fazety, délka 160mm","1ks",22.267499471146888,{"$f":"F5099*(1-Elteq!$F$9)","v":22.267499471146888},""]
["TECHNIK","KN 72 02 125",null,"7202125 KNIPEX kleště štípací stranové na plasty bez fazety, délka 125mm","1ks",22.675736961451246,{"$f":"F5100*(1-Elteq!$F$9)","v":22.675736961451246},""]
["TECHNIK","KN 72 11 160",null,"7211160 KNIPEX kleště štípací stranové na plasty bez fazety 45°, délka 160mm","1ks",35.108424166174927,{"$f":"F5101*(1-Elteq!$F$9)","v":35.108424166174927},""]
["TECHNIK","KN 72 51 160",null,"7251160 KNIPEX nůžky na optické vodiče, rukojeti potažené PVC, délka 160mm","1ks",26.23853687683475,{"$f":"F5102*(1-Elteq!$F$9)","v":26.23853687683475},""]
["TECHNIK","KN 73 72 180",null,"7372180 KNIPEX kleště štípací stranové silné, dvoukomponentní rukojeti, délka 180mm TwinForce","1ks",54.147136214005513,{"$f":"F5103*(1-Elteq!$F$9)","v":54.147136214005513},""]
["TECHNIK","KN 74 01 180",null,"7401180 KNIPEX kleště štípací stranové silné, rukojeti potažené PVC, délka 180mm","1ks",22.156161973791153,{"$f":"F5104*(1-Elteq!$F$9)","v":22.156161973791153},""]
["TECHNIK","KN 74 01 200",null,"7401200 KNIPEX kleště štípací stranové silné, rukojeti potažené PVC, délka 200mm","1ks",24.420024420024419,{"$f":"F5105*(1-Elteq!$F$9)","v":24.420024420024419},""]
["TECHNIK","KN 74 02 160",null,"7402160 KNIPEX kleště štípací stranové silné, dvoukomponentní rukojeti, délka 160mm","1ks",24.271574423550106,{"$f":"F5106*(1-Elteq!$F$9)","v":24.271574423550106},""]
["TECHNIK","KN 74 02 180",null,"7402180 KNIPEX kleště štípací stranové silné, dvoukomponentní rukojeti, délka 180mm","1ks",26.683886866257687,{"$f":"F5107*(1-Elteq!$F$9)","v":26.683886866257687},""]
["TECHNIK","KN 74 02 200",null,"7402200 KNIPEX kleště štípací stranové silné, dvoukomponentní rukojeti, délka 200mm","1ks",28.502399323068015,{"$f":"F5108*(1-Elteq!$F$9)","v":28.502399323068015},""]
["TECHNIK","KN 74 06 160",null,"7406160 KNIPEX kleště štípací stranové silné do 1000V, dvoukomponentní rukojeti, délka 160mm","1ks",32.955899217297393,{"$f":"F5109*(1-Elteq!$F$9)","v":32.955899217297393},""]
["TECHNIK","KN 74 06 180",null,"7406180 KNIPEX kleště štípací stranové silné do 1000V, dvoukomponentní rukojeti, délka 180mm","1ks",35.62799915383502,{"$f":"F5110*(1-Elteq!$F$9)","v":35.62799915383502},""]
["TECHNIK","KN 74 06 250",null,"7406250 KNIPEX kleště štípací stranové silné do 1000V, dvoukomponentní rukojeti, délka 250mm","1ks",46.056611406155476,{"$f":"F5111*(1-Elteq!$F$9)","v":46.056611406155476},""]
["TECHNIK","KN 74 12 180",null,"7412180 KNIPEX kleště štípací stranové silné s pružinou, dvoukomponentní rukojeti, délka 180mm","1ks",29.281761804558158,{"$f":"F5112*(1-Elteq!$F$9)","v":29.281761804558158},""]
["TECHNIK","KN 74 22 200",null,"7422200 KNIPEX kleště štípací stranové silné, fosfátované na černo a leštěné, délka 200mm","1ks",29.43021180103247,{"$f":"F5113*(1-Elteq!$F$9)","v":29.43021180103247},""]
["TECHNIK","KN 75 22 125",null,"7522125 KNIPEX kleště štípací stranové pro elektroniku, rukojeti potažené PVC, délka 125mm","1ks",36.036236644139379,{"$f":"F5114*(1-Elteq!$F$9)","v":36.036236644139379},""]
["TECHNIK","KN 75 52 125",null,"7552125 KNIPEX kleště štípací stranové pro elektroniku, rukojeti potažené PVC, délka 125mm","1ks",39.710374056878614,{"$f":"F5115*(1-Elteq!$F$9)","v":39.710374056878614},""]
["TECHNIK","KN 76 05 125",null,"7605125 KNIPEX kleště štípací malé s fazetou pro elektroniku, dvoukomponentní rukojeti","1ks",26.646774367139109,{"$f":"F5116*(1-Elteq!$F$9)","v":26.646774367139109},""]
["TECHNIK","KN 76 12 125",null,"7612125 KNIPEX kleště štípací malé s fazetou pro elektroniku, dvoukomponentní rukojeti","1ks",24.568474416498734,{"$f":"F5117*(1-Elteq!$F$9)","v":24.568474416498734},""]
["TECHNIK","KN 76 22 125",null,"7622125 KNIPEX kleště štípací malé bez fazety, dvoukomponentní rukojeti, délka 125mm","1ks",25.236499400633139,{"$f":"F5118*(1-Elteq!$F$9)","v":25.236499400633139},""]
["TECHNIK","KN 77 01 115",null,"7701115 KNIPEX kleště štípací malé s fazetou, rukojeti potažené PVC, délka 115mm","1ks",30.283799280759766,{"$f":"F5119*(1-Elteq!$F$9)","v":30.283799280759766},""]
["TECHNIK","KN 77 02 115",null,"7702115 KNIPEX kleště štípací malé s malou fazetou, dvoukomponentní rukojeti, délka 115mm","1ks",34.069274190854735,{"$f":"F5120*(1-Elteq!$F$9)","v":34.069274190854735},""]
["TECHNIK","KN 77 02 130",null,"7702130 KNIPEX kleště štípací malé s malou fazetou, dvoukomponentní rukojeti, délka 130mm","1ks",36.333136637088003,{"$f":"F5121*(1-Elteq!$F$9)","v":36.333136637088003},""]
["TECHNIK","KN 77 21 115",null,"7721115 KNIPEX kleště štípací malé bez fazety, rukojeti potažené PVC, délka 115mm","1ks",31.80541174462147,{"$f":"F5122*(1-Elteq!$F$9)","v":31.80541174462147},""]
["TECHNIK","KN 77 21 130",null,"7721130 KNIPEX kleště štípací malé bez fazety, rukojeti potažené PVC, délka 130mm","1ks",33.141461712890283,{"$f":"F5123*(1-Elteq!$F$9)","v":33.141461712890283},""]
["TECHNIK","KN 77 22 115",null,"7722115 KNIPEX kleště štípací malé bez fazety, dvoukomponentní rukojeti, délka 115mm","1ks",34.29194918556621,{"$f":"F5124*(1-Elteq!$F$9)","v":34.29194918556621},""]
["TECHNIK","KN 77 22 115 ESD",null,"7722115ESD KNIPEX kleště štípací malé bez fazety, antistatické provedení, délka 115mm","1ks",36.221799139732269,{"$f":"F5125*(1-Elteq!$F$9)","v":36.221799139732269},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"KN 77 22 130",null,"7722130 KNIPEX kleště štípací malé bez fazety, dvoukomponentní rukojeti, délka 130mm","1ks",36.444474134443738,{"$f":"F5126*(1-Elteq!$F$9)","v":36.444474134443738},""]
["TECHNIK","KN 77 32 115",null,"7732115 KNIPEX kleště štípací malé s fazetou, dvoukomponentní rukojeti, délka 115mm","1ks",37.557849108001086,{"$f":"F5127*(1-Elteq!$F$9)","v":37.557849108001086},""]
["TECHNIK","KN 77 42 115",null,"7742115 KNIPEX kleště štípací malé bez fazety, dvoukomponentní rukojeti, délka 115mm","1ks",36.555811631799472,{"$f":"F5128*(1-Elteq!$F$9)","v":36.555811631799472},""]
["TECHNIK","KN 77 72 115",null,"7772115 KNIPEX kleště štípací malé s fazetou, dvoukomponentní rukojeti, délka 115mm","1ks",36.555811631799472,{"$f":"F5129*(1-Elteq!$F$9)","v":36.555811631799472},""]
["TECHNIK","KN 78 03 125",null,"7803125 KNIPEX kleště štípací malé bez fazety PN1 inox, délka 125mm","1ks",19.335612040779214,{"$f":"F5130*(1-Elteq!$F$9)","v":19.335612040779214},""]
["TECHNIK","KN 78 13 125",null,"7813125 KNIPEX kleště štípací malé bez fazety PN1 inox s držením drátu, délka 125mm","1ks",21.747924483486795,{"$f":"F5131*(1-Elteq!$F$9)","v":21.747924483486795},""]
["TECHNIK","KN 78 61 125",null,"7861125 KNIPEX kleště štípací malé bez fazety PN1 brunýrované, délka 125mm","1ks",20.152087021387935,{"$f":"F5132*(1-Elteq!$F$9)","v":20.152087021387935},""]
["TECHNIK","KN 85 01 250",null,"8501250 KNIPEX kleště trubkové SMART GRIP, rukojeti potažené PVC, délka 250mm","1ks",42.97627397931349,{"$f":"F5133*(1-Elteq!$F$9)","v":42.97627397931349},""]
["TECHNIK","KN 85 51 250A",null,"8551250 KNIPEX kleště na hadicové spony, rukojeti potažené PVC, rozsah 0-70mm, délka 250mm","1ks",55.928536171697267,{"$f":"F5134*(1-Elteq!$F$9)","v":55.928536171697267},""]
["TECHNIK","KN 86 03 125",null,"8603125 KNIPEX kleště paralelní, niklované, rukojeti potažené PVC, rozsah 0-23mm, délka 125mm","1ks",41.417549016333211,{"$f":"F5135*(1-Elteq!$F$9)","v":41.417549016333211},""]
["TECHNIK","KN 86 03 150",null,"8603150 KNIPEX kleště paralelní, niklované, rukojeti potažené PVC, rozsah 0-27mm, délka 150mm","1ks",46.613298892934154,{"$f":"F5136*(1-Elteq!$F$9)","v":46.613298892934154},""]
["TECHNIK","KN 86 03 180",null,"8603180 KNIPEX kleště paralelní, niklované, rukojeti potažené PVC, rozsah 0-35mm, délka 180mm","1ks",48.765823841811681,{"$f":"F5137*(1-Elteq!$F$9)","v":48.765823841811681},""]
["TECHNIK","KN 86 03 250",null,"8603250 KNIPEX kleště paralelní, niklované, rukojeti potažené PVC, rozsah 0-46mm, délka 250mm","1ks",55.928536171697267,{"$f":"F5138*(1-Elteq!$F$9)","v":55.928536171697267},""]
["TECHNIK","KN 86 03 300",null,"8603300 KNIPEX kleště paralelní, niklované, rukojeti potažené PVC, rozsah 0-60mm, délka 300mm","1ks",66.245810926661989,{"$f":"F5139*(1-Elteq!$F$9)","v":66.245810926661989},""]
["TECHNIK","KN 86 03 400",null,"8603400 KNIPEX kleště paralelní, niklované, rukojeti potažené PVC, rozsah 0-85mm, délka 400mm","1ks",117.98063469795993,{"$f":"F5140*(1-Elteq!$F$9)","v":117.98063469795993},""]
["TECHNIK","KN 86 05 150",null,"8605150 KNIPEX kleště paralelní, niklované, dvoukomponentní rukojeti, rozsah 0-27mm, délka 150mm","1ks",50.176098808317654,{"$f":"F5141*(1-Elteq!$F$9)","v":50.176098808317654},""]
["TECHNIK","KN 86 05 180",null,"8605180 KNIPEX kleště paralelní, niklované, dvoukomponentní rukojeti, rozsah 0-35mm, délka 180mm","1ks",51.697711272179355,{"$f":"F5142*(1-Elteq!$F$9)","v":51.697711272179355},""]
["TECHNIK","KN 86 05 250",null,"8605250 KNIPEX kleště paralelní, niklované, dvoukomponentní rukojeti, rozsah 0-46mm, délka 250mm","1ks",59.862461078266548,{"$f":"F5143*(1-Elteq!$F$9)","v":59.862461078266548},""]
["TECHNIK","KN 86 07 250",null,"8607250 KNIPEX kleště paralelní, niklované, izolované do 1000V, rozsah 0-46mm, délka 250mm","1ks",69.029248360555357,{"$f":"F5144*(1-Elteq!$F$9)","v":69.029248360555357},""]
["TECHNIK","KN 87 01 125",null,"8701125 KNIPEX kleště trubkové COBRA, rukojeti potažené PVC, délka 125mm","1ks",22.156161973791153,{"$f":"F5145*(1-Elteq!$F$9)","v":22.156161973791153},""]
["TECHNIK","KN 87 01 150",null,"8701150 KNIPEX kleště trubkové COBRA, rukojeti potažené PVC, délka 150mm","1ks",22.490174465858356,{"$f":"F5146*(1-Elteq!$F$9)","v":22.490174465858356},""]
["TECHNIK","KN 87 01 180",null,"8701180 KNIPEX kleště trubkové COBRA, rukojeti potažené PVC, délka 180mm","1ks",23.640661938534279,{"$f":"F5147*(1-Elteq!$F$9)","v":23.640661938534279},""]
["TECHNIK","KN 87 01 250",null,"8701250 KNIPEX kleště trubkové COBRA, rukojeti potažené PVC, délka 250mm","1ks",25.236499400633139,{"$f":"F5148*(1-Elteq!$F$9)","v":25.236499400633139},""]
["TECHNIK","KN 87 01 300",null,"8701300 KNIPEX kleště trubkové COBRA, rukojeti potažené PVC, délka 300mm","1ks",34.663074176751991,{"$f":"F5149*(1-Elteq!$F$9)","v":34.663074176751991},""]
["TECHNIK","KN 87 01 400",null,"8701400 KNIPEX kleště trubkové COBRA, rukojeti potažené PVC, délka 400mm","1ks",60.382036065926641,{"$f":"F5150*(1-Elteq!$F$9)","v":60.382036065926641},""]
["TECHNIK","KN 87 01 560",null,"8701560 KNIPEX kleště trubkové COBRA, rukojeti potažené PVC, délka 560mm","1ks",100.50064761310962,{"$f":"F5151*(1-Elteq!$F$9)","v":100.50064761310962},""]
["TECHNIK","KN 87 02 180",null,"8702180 KNIPEX kleště trubkové COBRA, dvoukomponentní rukojeti, délka 180mm","1ks",26.23853687683475,{"$f":"F5152*(1-Elteq!$F$9)","v":26.23853687683475},""]
["TECHNIK","KN 87 02 250",null,"8702250 KNIPEX kleště trubkové COBRA, dvoukomponentní rukojeti, délka 250mm","1ks",28.168386831000813,{"$f":"F5153*(1-Elteq!$F$9)","v":28.168386831000813},""]
["TECHNIK","KN 87 02 300",null,"8702300 KNIPEX kleště trubkové COBRA, dvoukomponentní rukojeti, délka 300mm","1ks",39.339249065692833,{"$f":"F5154*(1-Elteq!$F$9)","v":39.339249065692833},""]
["TECHNIK","KN 87 05 250",null,"8705250 KNIPEX kleště trubkové COBRA, chromované, dvoukomponentní rukojeti, délka 250mm","1ks",36.630036630036628,{"$f":"F5155*(1-Elteq!$F$9)","v":36.630036630036628},""]
["TECHNIK","KN 87 05 300",null,"8705300 KNIPEX kleště trubkové COBRA, chromované, dvoukomponentní rukojeti, délka 300mm","1ks",47.281323877068559,{"$f":"F5156*(1-Elteq!$F$9)","v":47.281323877068559},""]
["TECHNIK","KN 87 26 250",null,"8726250 KNIPEX kleště trubkové COBRA, chromované, izolované do 1000V, délka 250mm","1ks",42.085574000467616,{"$f":"F5157*(1-Elteq!$F$9)","v":42.085574000467616},""]
["TECHNIK","KN 87 51 250",null,"8751250 KNIPEX kleště trubkové COBRA úzké, rukojeti potažené PVC, délka 250mm","1ks",26.015861882123279,{"$f":"F5158*(1-Elteq!$F$9)","v":26.015861882123279},""]
["TECHNIK","KN 88 01 180",null,"8801180 KNIPEX kleště trubkové ALIGATOR, rukojeti potažené PVC, délka 180mm","1ks",18.110899569866135,{"$f":"F5159*(1-Elteq!$F$9)","v":18.110899569866135},""]
["TECHNIK","KN 88 01 250",null,"8801250 KNIPEX kleště trubkové ALIGATOR, rukojeti potažené PVC, délka 250mm","1ks",19.335612040779214,{"$f":"F5160*(1-Elteq!$F$9)","v":19.335612040779214},""]
["TECHNIK","KN 88 01 300",null,"8801300 KNIPEX kleště trubkové ALIGATOR, rukojeti potažené PVC, délka 300mm","1ks",29.021974310728108,{"$f":"F5161*(1-Elteq!$F$9)","v":29.021974310728108},""]
["TECHNIK","KN 88 02 180",null,"8802180 KNIPEX kleště trubkové ALIGATOR, dvoukomponentní rukojeti, délka 180mm","1ks",20.894337003759496,{"$f":"F5162*(1-Elteq!$F$9)","v":20.894337003759496},""]
["TECHNIK","KN 88 02 250",null,"8802250 KNIPEX kleště trubkové ALIGATOR, dvoukomponentní rukojeti, délka 250mm","1ks",22.935524455281293,{"$f":"F5163*(1-Elteq!$F$9)","v":22.935524455281293},""]
["TECHNIK","KN 88 02 300",null,"8802300 KNIPEX kleště trubkové ALIGATOR, dvoukomponentní rukojeti, délka 300mm","1ks",31.285836756961377,{"$f":"F5164*(1-Elteq!$F$9)","v":31.285836756961377},""]
["TECHNIK","KN 88 06 250",null,"8806250 KNIPEX kleště trubkové ALIGATOR, chromované, izolované do 1000V, délka 250mm","1ks",33.030124215534549,{"$f":"F5165*(1-Elteq!$F$9)","v":33.030124215534549},""]
["TECHNIK","KN 92 02 53",null,"920253 KNIPEX pinzeta precizní zahnutá","1ks",19.59539953460926,{"$f":"F5166*(1-Elteq!$F$9)","v":19.59539953460926},""]
["TECHNIK","KN 92 22 07",null,"922207 KNIPEX pinzeta precizní špičatá rovná","1ks",14.176974663296852,{"$f":"F5167*(1-Elteq!$F$9)","v":14.176974663296852},""]
["TECHNIK","KN 92 27 61",null,"922761 KNIPEX pinzeta precizní rovná, izolovaná do 1000V","1ks",21.154124497589542,{"$f":"F5168*(1-Elteq!$F$9)","v":21.154124497589542},""]
["TECHNIK","KN 92 27 62",null,"922762 KNIPEX pinzeta precizní rovná, izolovaná do 1000V","1ks",21.228349495826699,{"$f":"F5169*(1-Elteq!$F$9)","v":21.228349495826699},""]
["TECHNIK","KN 92 28 69 ESD",null,"922869ESD KNIPEX pinzeta precizní špičatá, izolovaná s antistatickou ochranou","1ks",11.541987225877804,{"$f":"F5170*(1-Elteq!$F$9)","v":11.541987225877804},""]
["TECHNIK","KN 92 37 64",null,"923764 KNIPEX pinzeta precizní zahnutá, izolovaná do 1000V","1ks",21.636586986131061,{"$f":"F5171*(1-Elteq!$F$9)","v":21.636586986131061},""]
["TECHNIK","KN 92 38 75 ESD",null,"923875ESD KNIPEX pinzeta precizní špičatá, izolovaná s antistatickou ochranou","1ks",18.853149552237699,{"$f":"F5172*(1-Elteq!$F$9)","v":18.853149552237699},""]
["TECHNIK","KN 95 03 160 SB",null,"9503160 KNIPEX nůžky na KEVLAR vodiče, délka 160mm","1ks",46.316398899985529,{"$f":"F5173*(1-Elteq!$F$9)","v":46.316398899985529},""]
["TECHNIK","KN 95 05 140",null,"9505140 KNIPEX nůžky kombinované, délka 140mm","1ks",15.253237137735617,{"$f":"F5174*(1-Elteq!$F$9)","v":15.253237137735617},""]
["TECHNIK","KN 95 05 165",null,"9505165 KNIPEX nůžky na Al a Cu vodiče do průměru 10mm, délka 165mm","1ks",19.187162044304902,{"$f":"F5175*(1-Elteq!$F$9)","v":19.187162044304902},""]
["TECHNIK","KN 95 06 230",null,"9506230 KNIPEX nůžky na Al a Cu vodiče do průměru 16mm, izolované do 1000V","1ks",49.693636319776139,{"$f":"F5176*(1-Elteq!$F$9)","v":49.693636319776139},""]
["TECHNIK","KN 95 11 165",null,"9511165 KNIPEX nůžky na Al a Cu vodiče do průměru 16mm, potahované rukojeti (PN16/1)","1ks",27.055011857443468,{"$f":"F5177*(1-Elteq!$F$9)","v":27.055011857443468},""]
["TECHNIK","KN 95 12 165",null,"9512165 KNIPEX nůžky na Al a Cu vodiče do průměru 16mm, dvoukomponentní rukojeti (PN16)","1ks",29.875561790455407,{"$f":"F5178*(1-Elteq!$F$9)","v":29.875561790455407},""]
["TECHNIK","KN 95 12 200",null,"9512200 KNIPEX nůžky na Al a Cu vodiče do průměru 20mm, dvoukomponentní rukojeti (PN25)","1ks",48.134911356795854,{"$f":"F5179*(1-Elteq!$F$9)","v":48.134911356795854},""]
["TECHNIK","KN 95 16 165",null,"9516165 KNIPEX nůžky na Al a Cu vodiče do průměru 16mm, izolované do 1000V (PN16/1000)","1ks",43.124723975787802,{"$f":"F5180*(1-Elteq!$F$9)","v":43.124723975787802},""]
["TECHNIK","KN 95 17 200",null,"9517200 KNIPEX nůžky na Al a Cu vodiče do průměru 20mm, masivní rukojeti izolované do 1000V","1ks",59.491336087080768,{"$f":"F5181*(1-Elteq!$F$9)","v":59.491336087080768},"8591735045395"]
["TECHNIK","KN 95 22 165",null,"9522165 nůžky na Al a Cu vodiče do průměru 16mm, dvoukomponentní rukojeti s vratnou pružinou PN16/P","1ks",38.337211589491226,{"$f":"F5182*(1-Elteq!$F$9)","v":38.337211589491226},"8591735035266"]
["TECHNIK","KN 95 26 165",null,"9526165 KNIPEX nůžky na Al a Cu vodiče do průměru 16mm, izolované do 1000V s vratnou pružinou","1ks",51.40081127923073,{"$f":"F5183*(1-Elteq!$F$9)","v":51.40081127923073},"8591735045401"]
["TECHNIK","KN 95 61 190",null,"9561190 KNIPEX nůžky na FE do průměru 4-6mm, délka 190mm (PNFE3/5)","1ks",38.63411158243985,{"$f":"F5184*(1-Elteq!$F$9)","v":38.63411158243985},""]
["TECHNIK","KN 97 21 215",null,"9721215 KNIPEX kleště lisovací hobby na kabelové koncovky s izolací","1ks",21.117011998470964,{"$f":"F5185*(1-Elteq!$F$9)","v":21.117011998470964},""]
["TECHNIK","KN 97 21 215B",null,"9721215B KNIPEX kleště lisovací hobby na konektory bez izolace","1ks",22.490174465858356,{"$f":"F5186*(1-Elteq!$F$9)","v":22.490174465858356},""]
["TECHNIK","KN 97 21 215C",null,"9721215C KNIPEX kleště lisovací hobby na kabelové koncovky bez izolace","1ks",22.378836968502622,{"$f":"F5187*(1-Elteq!$F$9)","v":22.378836968502622},""]
["TECHNIK","KN 97 50 01",null,"975001 KNIPEX kleště lisovací pro konektory SCOTCHLOK (model KNIPEX, 3M nebo NO NAME)","1ks",35.999124145020801,{"$f":"F5188*(1-Elteq!$F$9)","v":35.999124145020801},"8591735040130"]
["TECHNIK","KN 97 51 10",null,"975110 KNIPEX kleště lisovací na telefonní a PC konektory RJ 11, 12 a 45","1ks",38.114536594779757,{"$f":"F5189*(1-Elteq!$F$9)","v":38.114536594779757},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"KN 97 51 12",null,"975112 KNIPEX kleště lisovací na telefonní a PC konektory RJ 10, 11, 12 a 45","1ks",123.65884706310239,{"$f":"F5190*(1-Elteq!$F$9)","v":123.65884706310239},""]
["TECHNIK","KN 97 52 05",null,"975205 KNIPEX lisovací kleště na neizolované konektory pro průřezy 0,5-6mm2 / šíře 4,8 a 6,3mm","1ks",128.96593443705905,{"$f":"F5191*(1-Elteq!$F$9)","v":128.96593443705905},"8591735056322"]
["TECHNIK","KN 97 52 06",null,"975206 KNIPEX lisovací kleště na izolované koncovky pro průřezy 0,5-6mm2","1ks",102.43049756727568,{"$f":"F5192*(1-Elteq!$F$9)","v":102.43049756727568},""]
["TECHNIK","KN 97 52 08",null,"975208 KNIPEX lisovací kleště na dutinky pro průřezy 0,25-6mm2","1ks",109.11074740861974,{"$f":"F5193*(1-Elteq!$F$9)","v":109.11074740861974},"8591735056315"]
["TECHNIK","KN 97 52 09",null,"975209 KNIPEX lisovací kleště na dutinky pro průřezy 10-25mm2","1ks",109.11074740861974,{"$f":"F5194*(1-Elteq!$F$9)","v":109.11074740861974},"8591735056346"]
["TECHNIK","KN 97 52 13",null,"975213 KNIPEX lisovací kleště na neizolovaná oka a spojky pro průřezy 0,5-10mm2","1ks",114.1209347896278,{"$f":"F5195*(1-Elteq!$F$9)","v":114.1209347896278},"8591735056339"]
["TECHNIK","KN 97 52 20",null,"975220 KNIPEX lisovací kleště na koaxiální konektory BNC, TNC, RG 58","1ks",143.06868410211877,{"$f":"F5196*(1-Elteq!$F$9)","v":143.06868410211877},"8591735048587"]
["TECHNIK","KN 97 53 09",null,"975309 KNIPEX kleště lisovací na dutinky pro průřezy 0,08-16mm2","1ks",168.04539600892184,{"$f":"F5197*(1-Elteq!$F$9)","v":168.04539600892184},"8591735036713"]
["TECHNIK","KN 97 61 145F",null,"9761145F KNIPEX kleště lisovací na dutinky o průřezu 0,25-2,5mm2 s vratnou pružinou","1ks",27.83437433893361,{"$f":"F5198*(1-Elteq!$F$9)","v":27.83437433893361},""]
["TECHNIK","HPH 1 crimpstar",null,"Lisovací kleště na oka a spojky se smršťovací bužírkou pro průřezy 0,5-6mm2, profi","1ks",107.06955995709795,{"$f":"F5199*(1-Elteq!$F$9)","v":107.06955995709795},""]
["TECHNIK","HX 1",null,"Lisovací kleště na koaxiální koncovky RG 55, 58, 59, 62, profi","1ks",44.534998942293775,{"$f":"F5200*(1-Elteq!$F$9)","v":44.534998942293775},"8591735008017"]
["TECHNIK","HX 1/TF",null,"Lisovací kleště na koaxiální koncovky RG 55, 58, 59, 62, robustní","1ks",65.317998448697537,{"$f":"F5201*(1-Elteq!$F$9)","v":65.317998448697537},"8591735041571"]
["TECHNIK","HX 2",null,"Lisovací kleště na koaxiální koncovky RG 8, 11, 213, profi","1ks",44.534998942293775,{"$f":"F5202*(1-Elteq!$F$9)","v":44.534998942293775},"8591735011635"]
["TECHNIK","HX 3",null,"Lisovací kleště na koaxiální koncovky RG 58, 59, 62, 6, profi","1ks",44.534998942293775,{"$f":"F5203*(1-Elteq!$F$9)","v":44.534998942293775},"8591735016395"]
["TECHNIK","HX 4",null,"Lisovací kleště na koaxiální koncovky LWL-SMA, B, C, MCX, profi","1ks",44.534998942293775,{"$f":"F5204*(1-Elteq!$F$9)","v":44.534998942293775},"8591735016401"]
["TECHNIK","HX 5",null,"Lisovací kleště na koaxiální koncovky RG174, 179, 8218 Fiber Optic, profi","1ks",44.534998942293775,{"$f":"F5205*(1-Elteq!$F$9)","v":44.534998942293775},"8591735041700"]
["TECHNIK","HX 6",null,"Lisovací kleště na koaxiální koncovky CATV F, RG 59, 6, profi","1ks",44.534998942293775,{"$f":"F5206*(1-Elteq!$F$9)","v":44.534998942293775},"8591735041816"]
["TECHNIK","HX 7",null,"Lisovací kleště na koaxiální koncovky CATV F, RG 59, 6, profi","1ks",44.534998942293775,{"$f":"F5207*(1-Elteq!$F$9)","v":44.534998942293775},"8591735041809"]
["TECHNIK","HX 8",null,"Lisovací kleště na koaxiální koncovky RG 59, 6, profi","1ks",44.534998942293775,{"$f":"F5208*(1-Elteq!$F$9)","v":44.534998942293775},"8591735050788"]
["TECHNIK","HX 9",null,"Lisovací kleště na koaxiální koncovky RG 58, 59, 6, 62, 142 profi","1ks",44.534998942293775,{"$f":"F5209*(1-Elteq!$F$9)","v":44.534998942293775},"8591735050795"]
["TECHNIK","LK1-DSK 08056",null,"Lisovací kleště na D-SUB konektory pro průřezy 0,03-0,56mm2","1ks",214.51024490538168,{"$f":"F5210*(1-Elteq!$F$9)","v":214.51024490538168},"8591735008048"]
["TECHNIK","LK1-DSK 08056 LOC",null,"Lisovací kleště s locatorem na D-SUB konektory pro průřezy 0,03-0,56mm2","1ks",308.96155516216305,{"$f":"F5211*(1-Elteq!$F$9)","v":308.96155516216305},"8591735048730"]
["TECHNIK","LK1-H&S 4",null,"Lisovací kleště na solární konektory Huber & Suhner pro průřezy 2,5-4mm2","1ks",203.74762016099402,{"$f":"F5212*(1-Elteq!$F$9)","v":203.74762016099402},"8591735032791"]
["TECHNIK","LK1-H&S 6",null,"Lisovací kleště na solární konektory Huber & Suhner pro průřezy 4-6mm2","1ks",203.74762016099402,{"$f":"F5213*(1-Elteq!$F$9)","v":203.74762016099402},"8591735032876"]
["TECHNIK","LK1-HIR",null,"Lisovací kleště na solární konektory Hirschmann SunCon pro průřezy 2,5-6mm2 ","1ks",203.74762016099402,{"$f":"F5214*(1-Elteq!$F$9)","v":203.74762016099402},"8591735032807"]
["TECHNIK","LK1-KK 01415",null,"Lisovací kleště na kruhové konektory pro průřezy 0,14-1,5mm2","1ks",216.36586986131059,{"$f":"F5215*(1-Elteq!$F$9)","v":216.36586986131059},"8591735008055"]
["TECHNIK","LK1-KOAX",null,"Lisovací kleště na koaxiální konektory RG 58, 59, 62, 71","1ks",178.51112076036088,{"$f":"F5216*(1-Elteq!$F$9)","v":178.51112076036088},"8591735041366"]
["TECHNIK","LK1-MC 3",null,"Lisovací kleště na solární konektory Multi-Contact MC3 pro průřezy 2,5-6mm2","1ks",215.62361987893902,{"$f":"F5217*(1-Elteq!$F$9)","v":215.62361987893902},"8591735032814"]
["TECHNIK","LK1-MC 3 LOC",null,"Lisovací kleště s locatorem na solární konektory Multi-Contact MC3 pro průřezy 2,5-6mm2","1ks",277.04480592018587,{"$f":"F5218*(1-Elteq!$F$9)","v":277.04480592018587},"8591735032821"]
["TECHNIK","LK1-MC 4",null,"Lisovací kleště na solární konektory Multi-Contact MC4 pro průřezy 2,5-6mm2","1ks",222.3038697202831,{"$f":"F5219*(1-Elteq!$F$9)","v":222.3038697202831},"8591735032838"]
["TECHNIK","LK1-MC 4 LOC",null,"Lisovací kleště s locatorem na solární konektory Multi-Contact MC4 pro průřezy 2,5-6mm2","1ks",283.91061825712279,{"$f":"F5220*(1-Elteq!$F$9)","v":283.91061825712279},"8591735056766"]
["TECHNIK","LK1-MC 4/4 UNI",null,"Multifunkční kleště s locatorem na solární konektory Multi-Contact MC4 pro průřezy 4mm2","1ks",365.74367881358762,{"$f":"F5221*(1-Elteq!$F$9)","v":365.74367881358762},"8591735032845"]
["TECHNIK","LK1-MC 4/6 UNI",null,"Multifunkční kleště s locatorem na solární konektory Multi-Contact MC4 pro průřezy 6mm2","1ks",365.74367881358762,{"$f":"F5222*(1-Elteq!$F$9)","v":365.74367881358762},"8591735032852"]
["TECHNIK","LK1-MK 0525",null,"Lisovací kleště na modulární konektory pro průřezy 0,5-2,5mm2","1ks",216.36586986131059,{"$f":"F5223*(1-Elteq!$F$9)","v":216.36586986131059},"8591735008079"]
["TECHNIK","LK1-MOJ 056 LOC",null,"Lisovací kleště s locatorem na konektory bez izolace s jazýčkem 0,5-6mm2, paralelní lisování","1ks",221.56161973791154,{"$f":"F5224*(1-Elteq!$F$9)","v":221.56161973791154},"8591735055073"]
["TECHNIK","LK1-SK 0144",null,"Lisovací kleště na soustružené kontakty pro průřezy 0,4-4mm2","1ks",147.70774649194101,{"$f":"F5225*(1-Elteq!$F$9)","v":147.70774649194101},"8591735008154"]
["TECHNIK","LK1-SK 0144 LOC",null,"Lisovací kleště s locatorem na soustružené kontakty pro průřezy 0,4-4mm2","1ks",322.87874233162989,{"$f":"F5226*(1-Elteq!$F$9)","v":322.87874233162989},"8591735048747"]
["TECHNIK","LK1-SK 156",null,"Lisovací kleště na soustružené kontakty pro průřezy 1,5-6mm2","1ks",219.33486979079683,{"$f":"F5227*(1-Elteq!$F$9)","v":219.33486979079683},"8591735008161"]
["TECHNIK","LK1-SK 156 LOC",null,"Lisovací kleště s locatorem na soustružené kontakty pro průřezy 1,5-6mm2","1ks",285.39511822186591,{"$f":"F5228*(1-Elteq!$F$9)","v":285.39511822186591},"8591735048754"]
["TECHNIK","LK1-SK 410",null,"Lisovací kleště na soustružené kontakty pro průřezy 4-10mm2","1ks",215.25249488775324,{"$f":"F5229*(1-Elteq!$F$9)","v":215.25249488775324},"8591735023331"]
["TECHNIK","LK1-SK 410 LOC",null,"Lisovací kleště s locatorem na soustružené kontakty pro průřezy 4-10mm2","1ks",276.85924342459299,{"$f":"F5230*(1-Elteq!$F$9)","v":276.85924342459299},"8591735048761"]
["TECHNIK","LK1-SK 625 LOC",null,"Lisovací kleště s locatorem na soustružené kontakty pro průřezy 6+25mm2","1ks",322.87874233162989,{"$f":"F5231*(1-Elteq!$F$9)","v":322.87874233162989},"8591735050139"]
["TECHNIK","LK1-SK1016 LOC",null,"Lisovací kleště s locatorem na soustružené kontakty pro průřezy 10-16mm2","1ks",324.36324229637302,{"$f":"F5232*(1-Elteq!$F$9)","v":324.36324229637302},"8591735050122"]
["TECHNIK","LK1-T/TM11",null,"Lisovací kleště na telefonní a PC konektory typu TM 11 HIROSE (625 30850 31) vč. kufru","1sada",403.41286541894442,{"$f":"F5233*(1-Elteq!$F$9)","v":403.41286541894442},"8591735042271"]
["TECHNIK","LK1-TYCO",null,"Lisovací kleště na solární konektory Tyco Solarlok pro průřezy 1,5-6mm2","1ks",279.82824335407923,{"$f":"F5234*(1-Elteq!$F$9)","v":279.82824335407923},"8591735032883"]
["TECHNIK","LK1-TYCO/LOC",null,"Lisovací kleště s locatorem na solární konektory Tyco Solarlok pro průřezy 1,5-6mm2","1ks",341.43499189091892,{"$f":"F5235*(1-Elteq!$F$9)","v":341.43499189091892},"8591735032890"]
["TECHNIK","LK-DSK 05075",null,"Lisovací kleště na D-SUB konektory pro průřezy 0,05-0,75mm2, economy","1ks",36.741374127392362,{"$f":"F5236*(1-Elteq!$F$9)","v":36.741374127392362},"8591735041854"]
["TECHNIK","LK-DSK 05075/P",null,"Lisovací kleště na D-SUB konektory pro průřezy 0,05-0,75mm2, profi","1ks",53.813123721938311,{"$f":"F5237*(1-Elteq!$F$9)","v":53.813123721938311},"8591735041861"]
["TECHNIK","LK-DSK 0805",null,"Lisovací kleště na D-SUB konektory pro průřezy 0,08-0,5mm2, economy","1ks",36.741374127392362,{"$f":"F5238*(1-Elteq!$F$9)","v":36.741374127392362},"8591735041830"]
["TECHNIK","LK-DSK 0805/P",null,"Lisovací kleště na D-SUB konektory pro průřezy 0,08-0,5mm2, profi","1ks",53.813123721938311,{"$f":"F5239*(1-Elteq!$F$9)","v":53.813123721938311},"8591735041847"]
["TECHNIK","LK-D-SUB",null,"Lisovací kleště na D-SUB konektory","1ks",18.370687063696181,{"$f":"F5240*(1-Elteq!$F$9)","v":18.370687063696181},"8591735023348"]
["TECHNIK","LK-MC 3",null,"Lisovací kleště na solární konektory Multi-Contact MC3 pro průřezy 2,5-6mm2, economy","1ks",61.606748536839724,{"$f":"F5241*(1-Elteq!$F$9)","v":61.606748536839724},"8591735041779"]
["TECHNIK","LK-MC 3/P",null,"Lisovací kleště na solární konektory Multi-Contact MC3 pro průřezy 2,5-6mm2, profi","1ks",75.709498201899422,{"$f":"F5242*(1-Elteq!$F$9)","v":75.709498201899422},"8591735035648"]
["TECHNIK","LK-MC 4",null,"Lisovací kleště na solární konektory Multi-Contact MC4 pro průřezy 6mm2, economy","1ks",61.606748536839724,{"$f":"F5243*(1-Elteq!$F$9)","v":61.606748536839724},"8591735041762"]
["TECHNIK","LK-MC 4/P",null,"Lisovací kleště na solární konektory Multi-Contact MC4 pro průřezy 6mm2, profi","1ks",75.709498201899422,{"$f":"F5244*(1-Elteq!$F$9)","v":75.709498201899422},"8591735035754"]
["TECHNIK","LK-MC 4/TF",null,"Lisovací kleště na solární konektory Multi-Contact MC4 pro průřezy 6mm2, profi","1ks",107.25512245269084,{"$f":"F5245*(1-Elteq!$F$9)","v":107.25512245269084},"8591735046545"]
["TECHNIK","LKS 0,03-0,56",null,"Lisovací kleště na soustružené kontakty pro průřezy 0,03-0,56mm2 s aplikátorem","1ks",342.91949185566205,{"$f":"F5246*(1-Elteq!$F$9)","v":342.91949185566205},"8591735050504"]
["TECHNIK","LKS 0,08-1,3",null,"Lisovací kleště na soustružené kontakty pro průřezy 0,08-1,3mm2 s aplikátorem","1ks",342.91949185566205,{"$f":"F5247*(1-Elteq!$F$9)","v":342.91949185566205},"8591735050498"]
["TECHNIK","LKS 0,08-2,5",null,"975264 KNIPEX lisovací kleště na soustružené kontakty pro průřezy 0,08-2,5mm2 s aplikátorem (LK-LK2)","1ks",514.75036277467893,{"$f":"F5248*(1-Elteq!$F$9)","v":514.75036277467893},"8591735016418"]
["TECHNIK","LKS 0,14-3,3",null,"Lisovací kleště na soustružené kontakty pro průřezy 0,14-3,3mm2 s aplikátorem","1ks",361.10461642376538,{"$f":"F5249*(1-Elteq!$F$9)","v":361.10461642376538},"8591735050511"]
["TECHNIK","LK-SIS 056",null,"Lisovací kleště na oka a spojky se smršťovací bužírkou pro průřezy 0,5-6mm2, economy","1ks",61.606748536839724,{"$f":"F5250*(1-Elteq!$F$9)","v":61.606748536839724},"8591735041724"]
["TECHNIK","LK-SIS 056/P",null,"Lisovací kleště na oka a spojky se smršťovací bužírkou pro průřezy 0,5-6mm2, profi","1ks",68.658123369369576,{"$f":"F5251*(1-Elteq!$F$9)","v":68.658123369369576},"8591735036539"]
["TECHNIK","LK-SIS 056/TF",null,"Lisovací kleště na oka a spojky se smršťovací bužírkou pro průřezy 0,5-6mm2, robustní","1ks",84.98762298154395,{"$f":"F5252*(1-Elteq!$F$9)","v":84.98762298154395},"8591735036522"]
["TECHNIK","LK-SK 01405",null,"Lisovací kleště na miniaturní D-SUB kontakty pro průřezy 0,14-0,5mm2","1ks",53.813123721938311,{"$f":"F5253*(1-Elteq!$F$9)","v":53.813123721938311},"8591735014025"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"LK-SK 054",null,"Lisovací kleště na miniaturní D-SUB kontakty pro průřezy 0,5-4mm2","1ks",53.813123721938311,{"$f":"F5254*(1-Elteq!$F$9)","v":53.813123721938311},"8591735032968"]
["TECHNIK","LK-T  4",null,"Lisovací kleště na telefonní a PC konektory 4-póly 4P4C (RJ10)","1ks",12.98937469150235,{"$f":"F5255*(1-Elteq!$F$9)","v":12.98937469150235},"8591735008802"]
["TECHNIK","LK-T  6",null,"Lisovací kleště na telefonní a PC konektory 6-pólů 6P4C, 6P6C (RJ11, RJ12)","1ks",12.98937469150235,{"$f":"F5256*(1-Elteq!$F$9)","v":12.98937469150235},"8591735008819"]
["TECHNIK","LK-T  8",null,"Lisovací kleště na telefonní a PC konektory 8-pólů 8P8C (RJ45)","1ks",12.98937469150235,{"$f":"F5257*(1-Elteq!$F$9)","v":12.98937469150235},"8591735008826"]
["TECHNIK","LK-T  8/TF",null,"Lisovací kleště na telefonní a PC konektory nestíněné 8P8C (RJ45) Stewart","1ks",81.276373069686144,{"$f":"F5258*(1-Elteq!$F$9)","v":81.276373069686144},"8591735038472"]
["TECHNIK","LK-T 10",null,"Lisovací kleště na telefonní a PC konektory 10-pólů 10P10C","1ks",16.700624603360165,{"$f":"F5259*(1-Elteq!$F$9)","v":16.700624603360165},"8591735035525"]
["TECHNIK","LK-T 10/E",null,"Lisovací kleště na telefonní a PC konektory 10-pólů 10P10C, economy","1ks",46.390623898222685,{"$f":"F5260*(1-Elteq!$F$9)","v":46.390623898222685},"8591735041717"]
["TECHNIK","LK-T 10/P",null,"Lisovací kleště na telefonní a PC konektory 10-pólů 10P10C, profi","1ks",69.400373351741138,{"$f":"F5261*(1-Elteq!$F$9)","v":69.400373351741138},"8591735041694"]
["TECHNIK","LK-T 46",null,"Lisovací kleště na telefonní a PC konektory 4-, 6-pólů 4P4C, 6P4C, 6P6C (RJ10, RJ11, RJ12)","1ks",21.896374479961107,{"$f":"F5262*(1-Elteq!$F$9)","v":21.896374479961107},"8591735008833"]
["TECHNIK","LK-T 68",null,"Lisovací kleště na telefonní a PC konektory 6-, 8-pólů 6P4C, 6P6C, 8P8C (RJ11, RJ12, RJ45)","1ks",21.896374479961107,{"$f":"F5263*(1-Elteq!$F$9)","v":21.896374479961107},"8591735008840"]
["TECHNIK","LK-T 68 P",null,"Lisovací kleště na telefonní a PC konektory 6-, 8-pólů 6P4C, 6P6C, 8P8C (RJ11, RJ12, RJ45), profi","1ks",36.926936622985252,{"$f":"F5264*(1-Elteq!$F$9)","v":36.926936622985252},"8591735020330"]
["TECHNIK","LK-T4610",null,"Lisovací kleště na telefonní a PC konektory 4-, 6-, 8-, 10-pólů","1ks",53.813123721938311,{"$f":"F5265*(1-Elteq!$F$9)","v":53.813123721938311},"8591735008857"]
["TECHNIK","LK-T468",null,"Lisovací kleště na telefonní a PC konektory 4-, 6-, 8-pólů","1ks",31.545624250791423,{"$f":"F5266*(1-Elteq!$F$9)","v":31.545624250791423},"8591735008864"]
["TECHNIK","LK-T468 A",null,"Lisovací kleště na telefonní a PC konektory 4-, 6-, 8-pólů, typ A","1ks",34.514624180277679,{"$f":"F5267*(1-Elteq!$F$9)","v":34.514624180277679},"8591735035532"]
["TECHNIK","LK-T468 H",null,"Lisovací kleště na telefonní a PC konektory 4-, 6-, 8-pólů, typ H","1ks",22.267499471146888,{"$f":"F5268*(1-Elteq!$F$9)","v":22.267499471146888},"8591735020323"]
["TECHNIK","LK-T468 P",null,"Lisovací kleště na telefonní a PC konektory 4-, 6-, 8-pólů, typ P","1ks",53.813123721938311,{"$f":"F5269*(1-Elteq!$F$9)","v":53.813123721938311},"8591735008871"]
["TECHNIK","LK-X1",null,"Lisovací kleště na koaxiální koncovky RG 58, 59, 62","1ks",24.123124427075794,{"$f":"F5270*(1-Elteq!$F$9)","v":24.123124427075794},"8591735008178"]
["TECHNIK","LK-X2",null,"Lisovací kleště na koaxiální koncovky RG 8, 11, 213","1ks",24.123124427075794,{"$f":"F5271*(1-Elteq!$F$9)","v":24.123124427075794},"8591735008185"]
["TECHNIK","LK-X3",null,"Lisovací kleště na koaxiální koncovky RG 58, 59, 62, 6","1ks",24.123124427075794,{"$f":"F5272*(1-Elteq!$F$9)","v":24.123124427075794},"8591735008192"]
["TECHNIK","LK-X4",null,"Lisovací kleště na koaxiální koncovky LWL-SMA, B, C, MCX","1ks",24.123124427075794,{"$f":"F5273*(1-Elteq!$F$9)","v":24.123124427075794},"8591735010768"]
["TECHNIK","LK-X5",null,"Lisovací kleště na koaxiální koncovky RG 174, 179, 8218","1ks",24.123124427075794,{"$f":"F5274*(1-Elteq!$F$9)","v":24.123124427075794},"8591735010775"]
["TECHNIK","LK-X6",null,"Lisovací kleště na koaxiální koncovky CATV F, RG59, RG6","1ks",24.123124427075794,{"$f":"F5275*(1-Elteq!$F$9)","v":24.123124427075794},"8591735041687"]
["TECHNIK","LK-X7",null,"Lisovací kleště na koaxiální koncovky CATV F, RG59, RG6","1ks",24.123124427075794,{"$f":"F5276*(1-Elteq!$F$9)","v":24.123124427075794},"8591735041670"]
["TECHNIK","LKZ-SK 156",null,"Lisovací kleště na soustružené kontakty pro průřezy 0,5-6mm2, zahnuté","1ks",26.720999365376265,{"$f":"F5277*(1-Elteq!$F$9)","v":26.720999365376265},"8591735049225"]
["TECHNIK","LOC1-DSK 08056",null,"974993 KNIPEX locator na D-SUB konektory 0,03-0,56mm2 ke kleštím LK1-DSK 08056","1ks",95.007997743560054,{"$f":"F5278*(1-Elteq!$F$9)","v":95.007997743560054},"8591735052553"]
["TECHNIK","LOC1-MC 3",null,"974972 KNIPEX locator na solární konektory Multi-Contact MC 3 ke kleštím LK1-MC3","1ks",63.833498483954408,{"$f":"F5279*(1-Elteq!$F$9)","v":63.833498483954408},"8591735040659"]
["TECHNIK","LOC1-MC 4",null,"974971 KNIPEX locator na solární konektory Multi-Contact MC 4 ke kleštím LK1-MC4","1ks",63.833498483954408,{"$f":"F5280*(1-Elteq!$F$9)","v":63.833498483954408},"8591735040666"]
["TECHNIK","LOC1-MO 056",null,"974995 KNIPEX locator na mosazné objímky 6,3mm ke kleštím LK1","1ks",32.658999224348769,{"$f":"F5281*(1-Elteq!$F$9)","v":32.658999224348769},"8591735049492"]
["TECHNIK","LOC1-MOJ 056",null,"Locator na mosazné objímky a kolíky s jazýčkem 6,3mm ke kleštím LK1","1ks",63.833498483954408,{"$f":"F5282*(1-Elteq!$F$9)","v":63.833498483954408},"8591735055042"]
["TECHNIK","LOC1-SK 0144",null,"974990 KNIPEX locator na soustružené kontakty 0,14-4mm2 ke kleštím LK1-SK 0144","1ks",101.31712259371834,{"$f":"F5283*(1-Elteq!$F$9)","v":101.31712259371834},"8591735028282"]
["TECHNIK","LOC1-TYCO",null,"9749681 KNIPEX locator na solární konektory Tyco Solarlok ke kleštím LK1-TYCO","1ks",63.833498483954408,{"$f":"F5284*(1-Elteq!$F$9)","v":63.833498483954408},"8591735040680"]
["TECHNIK","LOC-LS 0,14-6",null,"Locator - pozicioner na soustružené kontakty 0,14-6mm2 ke kleštím LS 0,14-6","1ks",63.833498483954408,{"$f":"F5285*(1-Elteq!$F$9)","v":63.833498483954408},"8591735040673"]
["TECHNIK","LS 0,08-2,5",null,"975263 KNIPEX lisovací kleště na soustružené kontakty pro průřezy 0,08-2,5mm2 bez locatoru","1ks",488.02936340930262,{"$f":"F5286*(1-Elteq!$F$9)","v":488.02936340930262},"8591735037932"]
["TECHNIK","LS 0,08-2,5 LOC",null,"975263 KNIPEX lisovací kleště na soustružené kontakty pro průřezy 0,08-2,5mm2 vč. locatoru","1ks",532.93548734278215,{"$f":"F5287*(1-Elteq!$F$9)","v":532.93548734278215},"8591735037949"]
["TECHNIK","LS 0,14-6",null,"975265 KNIPEX lisovací kleště na soustružené kontakty pro průřezy 0,14-6mm2 (LK-LK6)","1ks",551.12061191088549,{"$f":"F5288*(1-Elteq!$F$9)","v":551.12061191088549},"8591735016425"]
["TECHNIK","LS 0,14-6 LOC",null,"975265 KNIPEX lisovací kleště na soustružené kontakty pro průřezy 0,14-6mm2 vč. locatoru","1ks",620.5209852626266,{"$f":"F5289*(1-Elteq!$F$9)","v":620.5209852626266},"8591735050153"]
["TECHNIK","LS 1,5-10",null,"Lisovací kleště na soustružené kontakty pro průřezy 1,5-10mm2","1ks",551.12061191088549,{"$f":"F5290*(1-Elteq!$F$9)","v":551.12061191088549},"8591735038571"]
["TECHNIK","LXR 1",null,"975250 KNIPEX lisovací kleště na koaxiální koncovky RG 55, 58, 59, 62","1ks",127.66699696790882,{"$f":"F5291*(1-Elteq!$F$9)","v":127.66699696790882},""]
["TECHNIK","WC-100",null,"Lisovací kleště na kontakty pro průřezy 0,08-0,34mm2","1ks",416.21667761485389,{"$f":"F5292*(1-Elteq!$F$9)","v":416.21667761485389},""]
["TECHNIK","CRIMPIT F 4",null,"Lisovací kleště na dutinky pro průřezy 0,5-4mm2, pevné čelisti","1ks",136.94512174755337,{"$f":"F5293*(1-Elteq!$F$9)","v":136.94512174755337},"8591735023485"]
["TECHNIK","CRIMPIT F 6auto",null,"Lisovací kleště na dutinky pro průřezy 0,5-6mm2, automatické (PZ3)","1ks",165.44752107062138,{"$f":"F5294*(1-Elteq!$F$9)","v":165.44752107062138},"8591735023492"]
["TECHNIK","CRIMPIT F 6gyra",null,"Lisovací kleště na dutinky pro průřezy 0,25-6mm2, otočné čelisti (PZ6ROTO) Weidmüller 9014350000","1ks",155.09313381653809,{"$f":"F5295*(1-Elteq!$F$9)","v":155.09313381653809},"8591735023508"]
["TECHNIK","CRIMPIT F 6L",null,"Lisovací kleště na dutinky pro průřezy 0,5-6mm2, pevné čelisti (LD0,5-6/Z)","1ks",80.162998096128788,{"$f":"F5296*(1-Elteq!$F$9)","v":80.162998096128788},"8591735007805"]
["TECHNIK","CRIMPIT F16L",null,"Lisovací kleště na dutinky pro průřezy 6,0-16mm2, pevné čelisti (LD6-16/Z)","1ks",89.441122875773331,{"$f":"F5297*(1-Elteq!$F$9)","v":89.441122875773331},"8591735011642"]
["TECHNIK","CRIMPIT F25L",null,"Lisovací kleště na dutinky pro průřezy 6,0-25mm2, pevné čelisti (LD6-25/P)","1ks",105.39949749676194,{"$f":"F5298*(1-Elteq!$F$9)","v":105.39949749676194},"8591735011611"]
["TECHNIK","CRIMPIT F50EN",null,"Lisovací kleště na dutinky pro průřezy 25-50mm2, velmi robustní","1ks",192.79943292101348,{"$f":"F5299*(1-Elteq!$F$9)","v":192.79943292101348},""]
["TECHNIK","CRIMPIT F50L",null,"Lisovací kleště na dutinky pro průřezy 35-50mm2, pevné čelisti (LD35-50/P)","1ks",104.65724751439038,{"$f":"F5300*(1-Elteq!$F$9)","v":104.65724751439038},"8591735011628"]
["TECHNIK","D 150240",null,"Lisovací čelist na dutinky pro průřezy 150-240mm2 pro práci ve svěráku","1ks",251.99386901514561,{"$f":"F5301*(1-Elteq!$F$9)","v":251.99386901514561},"8591735023515"]
["TECHNIK","D 70150",null,"Lisovací čelist na dutinky pro průřezy 70-150mm2 pro práci ve svěráku","1ks",251.99386901514561,{"$f":"F5302*(1-Elteq!$F$9)","v":251.99386901514561},"8591735023522"]
["TECHNIK","FLEXI-CRIMP 6",null,"Lisovací kleště na dutinky pro průřezy 0,14-6mm2, délka 190mm, hmotnost 0,3kg  (Klauke K38/2)","1ks",93.523497778816932,{"$f":"F5303*(1-Elteq!$F$9)","v":93.523497778816932},"8591735013561"]
["TECHNIK","HNKE  4",null,"Lisovací kleště na dutinky pro průřezy 0,5-4mm2, trapéz, profi","1ks",35.25687416264924,{"$f":"F5304*(1-Elteq!$F$9)","v":35.25687416264924},"8591735023539"]
["TECHNIK","HNKE  4/TF",null,"Lisovací kleště na dutinky pro průřezy 0,5-4mm2, robustní","1ks",64.946873457511757,{"$f":"F5305*(1-Elteq!$F$9)","v":64.946873457511757},"8591735023546"]
["TECHNIK","HNKE  6",null,"Lisovací kleště na dutinky pro průřezy 0,5-6mm2, trapéz, profi","1ks",35.25687416264924,{"$f":"F5306*(1-Elteq!$F$9)","v":35.25687416264924},"8591735035617"]
["TECHNIK","HNKE  6/TF",null,"Lisovací kleště na dutinky pro průřezy 0,5-6mm2, robustní","1ks",68.658123369369576,{"$f":"F5307*(1-Elteq!$F$9)","v":68.658123369369576},"8591735041151"]
["TECHNIK","HNKE  616",null,"Lisovací kleště na dutinky pro průřezy 6,0-16mm2, trapéz, profi","1ks",35.25687416264924,{"$f":"F5308*(1-Elteq!$F$9)","v":35.25687416264924},"8591735035624"]
["TECHNIK","HNKE  6U6",null,"975314 KNIPEX lisovací kleště na dutinky pro průřezy 0,08-6mm2, šestihran (LDU)","1ks",169.04743348512346,{"$f":"F5309*(1-Elteq!$F$9)","v":169.04743348512346},"8591735016371"]
["TECHNIK","HNKE 02516",null,"Lisovací kleště na dutinky pro průřezy 0,25-16mm2, profi","1ks",73.853873245970505,{"$f":"F5310*(1-Elteq!$F$9)","v":73.853873245970505},"8591735041823"]
["TECHNIK","HNKE 02516/TF",null,"Lisovací kleště na dutinky pro průřezy 0,25-16mm2, robustní","1ks",81.276373069686144,{"$f":"F5311*(1-Elteq!$F$9)","v":81.276373069686144},"8591735054557"]
["TECHNIK","HNKE 10P",null,"975308 KNIPEX lisovací kleště na dutinky pro průřezy 0,08-10mm2, čtyřhran, profi","1ks",163.10943362615095,{"$f":"F5312*(1-Elteq!$F$9)","v":163.10943362615095},"8591735007713"]
["TECHNIK","HNKE 10U6",null,"975314 KNIPEX lisovací kleště na dutinky pro průřezy 0,08-10mm2, šestihran (LDU)","1ks",172.75868339698127,{"$f":"F5313*(1-Elteq!$F$9)","v":172.75868339698127},"8591735052522"]
["TECHNIK","HNKE 16",null,"Lisovací kleště na dutinky pro průřezy 0,5-16mm2, trapéz, profi","1ks",36.741374127392362,{"$f":"F5314*(1-Elteq!$F$9)","v":36.741374127392362},"8591735007751"]
["TECHNIK","HNKE 16/TF",null,"Lisovací kleště na dutinky pro průřezy 0,5-16mm2, robustní","1ks",70.142623334112699,{"$f":"F5315*(1-Elteq!$F$9)","v":70.142623334112699},"8591735023553"]
["TECHNIK","HNKE 1635",null,"Lisovací kleště na dutinky pro průřezy 16-35mm2, široký trapéz","1ks",35.25687416264924,{"$f":"F5316*(1-Elteq!$F$9)","v":35.25687416264924},"8591735041656"]
["TECHNIK","HNKE 16P",null,"975309 KNIPEX lisovací kleště na dutinky pro průřezy 0,08-16mm2, čtyřhran, profi","1ks",199.29412026676465,{"$f":"F5317*(1-Elteq!$F$9)","v":199.29412026676465},"8591735016388"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"HNKE 16U",null,"975304 KNIPEX lisovací kleště na dutinky pro průřezy 0,08-16mm2, čtyřhran (LDU) dříve HNKE10U","1ks",153.46018385532062,{"$f":"F5318*(1-Elteq!$F$9)","v":153.46018385532062},"8591735052515"]
["TECHNIK","HNKE 25/50",null,"Lisovací kleště na dutinky pro průřezy 25 a 50mm2, profi","1ks",35.25687416264924,{"$f":"F5319*(1-Elteq!$F$9)","v":35.25687416264924},"8591735012953"]
["TECHNIK","HNKE 25/50/TF",null,"Lisovací kleště na dutinky pro průřezy 25 a 50mm2, robustní","1ks",70.142623334112699,{"$f":"F5320*(1-Elteq!$F$9)","v":70.142623334112699},"8591735023560"]
["TECHNIK","HNKE 35",null,"Lisovací kleště na dutinky pro průřezy 16-35mm2, profi","1ks",35.25687416264924,{"$f":"F5321*(1-Elteq!$F$9)","v":35.25687416264924},"8591735012960"]
["TECHNIK","HNKE 35/TF",null,"Lisovací kleště na dutinky pro průřezy 16-35mm2, robustní","1ks",70.142623334112699,{"$f":"F5322*(1-Elteq!$F$9)","v":70.142623334112699},"8591735023577"]
["TECHNIK","HNKE 50 crimpstar",null,"Lisovací kleště na dutinky pro průřezy 25-50mm2, crimpstar","1ks",117.27549721470695,{"$f":"F5323*(1-Elteq!$F$9)","v":117.27549721470695},"8591735007720"]
["TECHNIK","HNKE 50L",null,"Lisovací kleště na dutinky pro průřezy 25-50mm2, profi","1ks",73.853873245970505,{"$f":"F5324*(1-Elteq!$F$9)","v":73.853873245970505},"8591735038168"]
["TECHNIK","HNKE 50L/TF",null,"Lisovací kleště na dutinky pro průřezy 25-50mm2, robustní","1ks",84.245372999172389,{"$f":"F5325*(1-Elteq!$F$9)","v":84.245372999172389},"8591735041465"]
["TECHNIK","JOKARI Q",null,"Lisovací kleště se zásobníkem na dutinky pro průřezy 0,5-2,5mm2 JOKARI","1ks",227.49961959688403,{"$f":"F5326*(1-Elteq!$F$9)","v":227.49961959688403},"8591735037796"]
["TECHNIK","JOKARI Q SET",null,"Lisovací kleště se zásobníkem na dutinky pro průřezy 0,5-2,5mm2 v kufru s příslušenstvím JOKARI","1sada",263.68430623749771,{"$f":"F5327*(1-Elteq!$F$9)","v":263.68430623749771},"8591735037802"]
["TECHNIK","KY-D 056",null,"Lisovací kleště na dutinky pro průřezy 0,5-6mm2, delší rukojeti","1ks",57.524373633796124,{"$f":"F5328*(1-Elteq!$F$9)","v":57.524373633796124},"8591735037789"]
["TECHNIK","KY-D 35",null,"Lisovací kleště na dutinky pro průřezy 16-35mm2, delší rukojeti","1ks",57.524373633796124,{"$f":"F5329*(1-Elteq!$F$9)","v":57.524373633796124},"8591735052867"]
["TECHNIK","LD 0,14-2,5",null,"Lisovací kleště na dutinky pro průřezy 0,14-2,5mm2, zahnuté","1ks",21.525249488775323,{"$f":"F5330*(1-Elteq!$F$9)","v":21.525249488775323},"8591735023584"]
["TECHNIK","LD 0,25-6",null,"Lisovací kleště na dutinky pro průřezy 0,25-6mm2, zahnuté","1ks",21.525249488775323,{"$f":"F5331*(1-Elteq!$F$9)","v":21.525249488775323},"8591735023591"]
["TECHNIK","LDR 0256",null,"975238 KNIPEX lisovací kleště na dutinky pro průřezy 0,25-6mm2","1ks",100.57487261134678,{"$f":"F5332*(1-Elteq!$F$9)","v":100.57487261134678},"8591735033477"]
["TECHNIK","LDR 1025",null,"Lisovací kleště na dutinky pro průřezy 10-25mm2, kvalitní Knipex","1ks",100.57487261134678,{"$f":"F5333*(1-Elteq!$F$9)","v":100.57487261134678},"8591735033484"]
["TECHNIK","LDZ 6-16",null,"Lisovací kleště na dutinky pro průřezy 6,0-16mm2, zahnuté","1ks",21.525249488775323,{"$f":"F5334*(1-Elteq!$F$9)","v":21.525249488775323},"8591735023607"]
["TECHNIK","LK1-D0256",null,"Lisovací kleště na dutinky pro průřezy 0,25-6mm2, paralelní lisování","1ks",143.43980909330455,{"$f":"F5335*(1-Elteq!$F$9)","v":143.43980909330455},"8591735032746"]
["TECHNIK","LK1-D1025",null,"Lisovací kleště na dutinky pro průřezy 10-25mm2, paralelní lisování","1ks",143.43980909330455,{"$f":"F5336*(1-Elteq!$F$9)","v":143.43980909330455},"8591735032753"]
["TECHNIK","LK1-D3550",null,"Lisovací kleště na dutinky pro průřezy 35-50mm2, paralelní lisování","1ks",178.1399957691751,{"$f":"F5337*(1-Elteq!$F$9)","v":178.1399957691751},"8591735032760"]
["TECHNIK","LK1-D70",null,"Lisovací kleště na dutinky pro průřezy 70mm2, paralelní lisování","1ks",197.43849531083575,{"$f":"F5338*(1-Elteq!$F$9)","v":197.43849531083575},"8591735032777"]
["TECHNIK","LK1-D95",null,"Lisovací kleště na dutinky pro průřezy 95mm2, paralelní lisování","1ks",197.43849531083575,{"$f":"F5339*(1-Elteq!$F$9)","v":197.43849531083575},"8591735032784"]
["TECHNIK","LK-D 02516",null,"9771180 KNIPEX lisovací kleště na dutinky pro průřezy 0,25-16mm2, rukojeti potažené PVC","1ks",30.432249277234078,{"$f":"F5340*(1-Elteq!$F$9)","v":30.432249277234078},"8591735007812"]
["TECHNIK","LK-D 02516 P",null,"9772180 KNIPEX lisovací kleště na dutinky pro průřezy 0,25-16mm2, dvoukomponentní rukojeti","1ks",33.475474204957486,{"$f":"F5341*(1-Elteq!$F$9)","v":33.475474204957486},"8591735007768"]
["TECHNIK","LK-D 02516/1000",null,"9778180 KNIPEX lisovací kleště na dutinky pro průřezy 0,25-16mm2, dvoukomponentní rukojeti do 1000V","1ks",35.553774155597864,{"$f":"F5342*(1-Elteq!$F$9)","v":35.553774155597864},""]
["TECHNIK","LK-D 02525",null,"Lisovací kleště na dutinky pro průřezy 0,25-2,5mm2, economy","1ks",15.587249629802821,{"$f":"F5343*(1-Elteq!$F$9)","v":15.587249629802821},"8591735048860"]
["TECHNIK","LK-D 02525/2",null,"Lisovací kleště na dutinky pro průřezy 0,25-2,5mm2, hobby","1ks",14.659437151838368,{"$f":"F5344*(1-Elteq!$F$9)","v":14.659437151838368},"8591735007782"]
["TECHNIK","LK-D 0256",null,"Lisovací kleště na dutinky pro průřezy 0,25-6mm2, čtyřhran (LDU 0,5-6) economy","1ks",44.534998942293775,{"$f":"F5345*(1-Elteq!$F$9)","v":44.534998942293775},"8591735007799"]
["TECHNIK","LK-D 0256U6",null,"Lisovací kleště na dutinky pro průřezy 0,25-6mm2, šestihran (LDU 0,5-6/6) economy","1ks",73.853873245970505,{"$f":"F5346*(1-Elteq!$F$9)","v":73.853873245970505},"8591735029401"]
["TECHNIK","LK-D 0516",null,"Lisovací kleště na dutinky pro průřezy 0,25-16mm2, economy","1ks",18.370687063696181,{"$f":"F5347*(1-Elteq!$F$9)","v":18.370687063696181},"8591735027094"]
["TECHNIK","LK-D 0516/2",null,"Lisovací kleště na dutinky pro průřezy 0,5-16mm2, hobby","1ks",18.370687063696181,{"$f":"F5348*(1-Elteq!$F$9)","v":18.370687063696181},"8591735007829"]
["TECHNIK","LK-D 0525",null,"9761145A KNIPEX lisovací kleště na dutinky pro průřezy 0,25-2,5mm2, economy","1ks",20.411874515217981,{"$f":"F5349*(1-Elteq!$F$9)","v":20.411874515217981},"8591735007836"]
["TECHNIK","LK-D 0525 P",null,"9762145A KNIPEX lisovací kleště na dutinky pro průřezy 0,25-2,5mm2, dvoukomponentní rukojeti","1ks",25.681849390056076,{"$f":"F5350*(1-Elteq!$F$9)","v":25.681849390056076},"8591735025380"]
["TECHNIK","LK-D 0525 P/1000",null,"9768145A KNIPEX lisovací kleště na dutinky pro průřezy 0,25-2,5mm2, dvoukomponentní rukojeti do1000V","1ks",26.869449361850577,{"$f":"F5351*(1-Elteq!$F$9)","v":26.869449361850577},"8591735055103"]
["TECHNIK","LK-D 054",null,"Lisovací kleště na dutinky pro průřezy 0,5-4mm2, economy","1ks",24.123124427075794,{"$f":"F5352*(1-Elteq!$F$9)","v":24.123124427075794},"8591735007683"]
["TECHNIK","LK-D 056",null,"9781180 KNIPEX lisovací kleště na dutinky pro průřezy 0,5-6mm2, rukojeti potažené PVC","1ks",45.054573929953868,{"$f":"F5353*(1-Elteq!$F$9)","v":45.054573929953868},"8591735007256"]
["TECHNIK","LK-D 07510",null,"Lisovací kleště na dutinky pro průřezy 0,75-10mm2, čtyřhran (LDU 1,0-10) economy","1ks",44.906123933479556,{"$f":"F5354*(1-Elteq!$F$9)","v":44.906123933479556},"8591735007850"]
["TECHNIK","LK-D 0810",null,"Lisovací kleště na dutinky pro průřezy 0,08-10mm2, délka 195mm, hmotnost 0,29kg (Klauke K30/3) profi","1ks",110.96637236454866,{"$f":"F5355*(1-Elteq!$F$9)","v":110.96637236454866},"8591735011093"]
["TECHNIK","LK-D 1035",null,"Lisovací kleště na dutinky pro průřezy 10-35mm2, economy","1ks",20.411874515217981,{"$f":"F5356*(1-Elteq!$F$9)","v":20.411874515217981},"8591735048853"]
["TECHNIK","LK-D 1050",null,"Lisovací kleště na dutinky pro průřezy 10-50mm2, (Klauke K28) profi","1ks",192.05718293864192,{"$f":"F5357*(1-Elteq!$F$9)","v":192.05718293864192},"8591735007737"]
["TECHNIK","LK-D 1050 E",null,"Lisovací kleště na dutinky pro průřezy 10-50mm2, economy","1ks",146.22324652719789,{"$f":"F5358*(1-Elteq!$F$9)","v":146.22324652719789},"8591735023614"]
["TECHNIK","LK-D 120150 E",null,"Lisovací kleště na dutinky pro průřezy 120-150mm2, economy","1ks",157.72812125395711,{"$f":"F5359*(1-Elteq!$F$9)","v":157.72812125395711},"8591735023621"]
["TECHNIK","LK-D 156",null,"Lisovací kleště na dutinky pro průřezy 1,5-6mm2, economy","1ks",17.071749594545945,{"$f":"F5360*(1-Elteq!$F$9)","v":17.071749594545945},"8591735048877"]
["TECHNIK","LK-D 1650",null,"Lisovací kleště na dutinky pro průřezy 16-50mm2, economy, modré","1ks",61.792311032432615,{"$f":"F5361*(1-Elteq!$F$9)","v":61.792311032432615},"8591735007881"]
["TECHNIK","LK-D 2516",null,"Lisovací kleště na dutinky pro průřezy 2,5-16mm2, délka 195mm, hmotnost 0,29kg (Klauke K30/4) profi","1ks",120.43005963978608,{"$f":"F5362*(1-Elteq!$F$9)","v":120.43005963978608},"8591735023645"]
["TECHNIK","LK-D 416",null,"Lisovací kleště na dutinky pro průřezy 4,0-16mm2, čtyřhran (LDU 4-16) economy","1ks",45.277248924665336,{"$f":"F5363*(1-Elteq!$F$9)","v":45.277248924665336},"8591735008086"]
["TECHNIK","LK-D 5095",null,"Lisovací kleště na dutinky pro průřezy 50-95mm2, profi (Klauke K29)","1ks",192.05718293864192,{"$f":"F5364*(1-Elteq!$F$9)","v":192.05718293864192},"8591735007744"]
["TECHNIK","LK-D 5095 E",null,"Lisovací kleště na dutinky pro průřezy 50-95mm2, economy","1ks",146.22324652719789,{"$f":"F5365*(1-Elteq!$F$9)","v":146.22324652719789},"8591735023638"]
["TECHNIK","LK-D 6",null,"Lisovací kleště na dutinky pro průřezy 0,5-6mm2, economy","1ks",24.123124427075794,{"$f":"F5366*(1-Elteq!$F$9)","v":24.123124427075794},"8591735038557"]
["TECHNIK","LK-D 616",null,"Lisovací kleště na dutinky pro průřezy 6,0-16mm2, economy","1ks",24.123124427075794,{"$f":"F5367*(1-Elteq!$F$9)","v":24.123124427075794},"8591735007904"]
["TECHNIK","LKZ-D 054",null,"Lisovací kleště na dutinky s izolací i bez izolace pro průřezy 0,5-4mm2, zahnuté (LDF0,5-4)","1ks",24.494249418261575,{"$f":"F5368*(1-Elteq!$F$9)","v":24.494249418261575},"8591735049010"]
["TECHNIK","LKZ-D 056",null,"Lisovací kleště na dutinky s izolací i bez izolace pro průřezy 0,5-6mm2, zahnuté (LDF0,5-6)","1ks",24.494249418261575,{"$f":"F5369*(1-Elteq!$F$9)","v":24.494249418261575},"8591735049027"]
["TECHNIK","LKZ-D 056/OI 0525",null,"Lisovací kleště na dutinky 0,5-6mm2 a izolované koncovky 0,5-2,5mm2, zahnuté (LDIF0,5-6/0,5-2,5)","1ks",26.720999365376265,{"$f":"F5370*(1-Elteq!$F$9)","v":26.720999365376265},"8591735049089"]
["TECHNIK","LKZ-D 1025",null,"Lisovací kleště na dutinky s izolací i bez izolace pro průřezy 10-25mm2 zahnuté (LDF10-25)","1ks",24.494249418261575,{"$f":"F5371*(1-Elteq!$F$9)","v":24.494249418261575},"8591735049058"]
["TECHNIK","LKZ-D 1035",null,"Lisovací kleště na dutinky s izolací i bez izolace pro průřezy 10-35mm2, zahnuté (LDF10-35)","1ks",26.720999365376265,{"$f":"F5372*(1-Elteq!$F$9)","v":26.720999365376265},"8591735049065"]
["TECHNIK","LKZ-D 110",null,"Lisovací kleště na dutinky s izolací i bez izolace pro průřezy 1,0-10mm2, zahnuté (LDF4-10)","1ks",24.494249418261575,{"$f":"F5373*(1-Elteq!$F$9)","v":24.494249418261575},"8591735049034"]
["TECHNIK","LKZ-D 2550",null,"Lisovací kleště na dutinky s izolací i bez izolace pro průřezy 25-50mm2, zahnuté (LDF25-50)","1ks",26.720999365376265,{"$f":"F5374*(1-Elteq!$F$9)","v":26.720999365376265},"8591735049072"]
["TECHNIK","LKZ-D 616",null,"Lisovací kleště na dutinky s izolací i bez izolace pro průřezy 6-16mm2, zahnuté (LDF6-16)","1ks",24.494249418261575,{"$f":"F5375*(1-Elteq!$F$9)","v":24.494249418261575},"8591735049041"]
["TECHNIK","PZ 1,5",null,"Lisovací kleště na dutinky pro průřezy 0,5-1,5mm2, profesionální Weidmüller 9005990000","1ks",90.406047852856361,{"$f":"F5376*(1-Elteq!$F$9)","v":90.406047852856361},""]
["TECHNIK","PZ 10 HEX",null,"Lisovací kleště na dutinky pro průřezy 0,14-10mm2, profesionální Weidmüller 1445070000","1ks",168.63919599481909,{"$f":"F5377*(1-Elteq!$F$9)","v":168.63919599481909},"8591735056995"]
["TECHNIK","PZ 10 SQR",null,"Lisovací kleště na dutinky pro průřezy 0,14-10mm2, profesionální Weidmüller 1445080000","1ks",168.63919599481909,{"$f":"F5378*(1-Elteq!$F$9)","v":168.63919599481909},"8591735056988"]
["TECHNIK","STRIPAX PLUS",null,"Odizolovací kleště s lisováním dutinek v páscích pro průřezy 0,5-2,5mm2","1ks",267.9522436361342,{"$f":"F5379*(1-Elteq!$F$9)","v":267.9522436361342},"8591735007706"]
["TECHNIK","WE300",null,"Odizolovací kleště s lisováním dutinek pro průřezy 0,5-6mm2 Duo Crimp","1ks",54.926498695495653,{"$f":"F5380*(1-Elteq!$F$9)","v":54.926498695495653},"8591735008918"]
["TECHNIK","HF 0525",null,"Lisovací kleště na konektory bez izolace pro průřezy 0,5-2,5mm2, profi","1ks",57.524373633796124,{"$f":"F5381*(1-Elteq!$F$9)","v":57.524373633796124},"8591735041649"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"HF 1",null,"Lisovací kleště na konektory bez izolace pro průřezy 0,5-6mm2, profi","1ks",44.534998942293775,{"$f":"F5382*(1-Elteq!$F$9)","v":44.534998942293775},"8591735007911"]
["TECHNIK","HF 1 crimpstar",null,"Lisovací kleště na konektory bez izolace pro průřezy 0,5-6mm2, crimpstar","1ks",164.96505858207985,{"$f":"F5383*(1-Elteq!$F$9)","v":164.96505858207985},""]
["TECHNIK","HF 1/TF",null,"Lisovací kleště na konektory bez izolace pro průřezy 0,5-6mm2, robustní","1ks",73.853873245970505,{"$f":"F5384*(1-Elteq!$F$9)","v":73.853873245970505},"8591735023126"]
["TECHNIK","HF 2",null,"975234 KNIPEX lisovací kleště na konektory bez izolace pro průřezy 0,1-2,5mm2","1ks",118.75999717945007,{"$f":"F5385*(1-Elteq!$F$9)","v":118.75999717945007},"8591735007928"]
["TECHNIK","HF 2/Z",null,"Lisovací kleště na konektory bez izolace pro průřezy 0,1-1,5 mm2, šíře 2,8 a 4,8mm (LK2/Z)","1ks",138.24405921670359,{"$f":"F5386*(1-Elteq!$F$9)","v":138.24405921670359},"8591735017668"]
["TECHNIK","HF 2/Z/LOC",null,"Lisovací kleště s locatorem na konektory bez izolace pro průřezy 0,1-1,5 mm2, šíře 2,8 a 4,8mm","1ks",166.07843355563719,{"$f":"F5387*(1-Elteq!$F$9)","v":166.07843355563719},""]
["TECHNIK","HF 3",null,"Lisovací kleště na konektory bez izolace pro průřezy 0,5-6mm2, šíře 4,8 a 6,3mm (Klauke K59/2)","1ks",109.66743489539842,{"$f":"F5388*(1-Elteq!$F$9)","v":109.66743489539842},"8591735011109"]
["TECHNIK","HF-BP",null,"Lisovací kleště na konektory bez izolace pro průřezy 0,1-6mm2, s bočním připojením 1,5-2,5mm2","1ks",223.78836968502623,{"$f":"F5389*(1-Elteq!$F$9)","v":223.78836968502623},"8591735007935"]
["TECHNIK","LK  2/Z",null,"Lisovací kleště na konektory bez izolace 0,1-1,5mm2","1ks",151.79012139498462,{"$f":"F5390*(1-Elteq!$F$9)","v":151.79012139498462},""]
["TECHNIK","LK 0,1-1",null,"Lisovací kleště na konektory bez izolace 0,1-1,0mm2 / šíře 2,8mm, zahnuté","1ks",21.525249488775323,{"$f":"F5391*(1-Elteq!$F$9)","v":21.525249488775323},"8591735023225"]
["TECHNIK","LK 0,14-1,5",null,"Lisovací kleště na konektory bez izolace 0,14-1,5mm2 / šíře 2,8 a 4,8mm, zahnuté","1ks",21.525249488775323,{"$f":"F5392*(1-Elteq!$F$9)","v":21.525249488775323},"8591735023218"]
["TECHNIK","LK 0,5-2,5",null,"Lisovací kleště na konektory bez izolace 0,5-2,5mm2 / šíře 4,8 a 6,3mm, zahnuté","1ks",21.525249488775323,{"$f":"F5393*(1-Elteq!$F$9)","v":21.525249488775323},"8591735023232"]
["TECHNIK","LK1-BP 051",null,"Lisovací kleště na objímky bez izolace s bočním připojením 0,5-1,0mm2","1ks",267.76668114054132,{"$f":"F5394*(1-Elteq!$F$9)","v":267.76668114054132},"8591735023249"]
["TECHNIK","LK1-BP 1525",null,"Lisovací kleště na objímky bez izolace s bočním připojením 1,25-2,5mm2","1ks",271.663493547992,{"$f":"F5395*(1-Elteq!$F$9)","v":271.663493547992},"8591735023256"]
["TECHNIK","LK1-MO 0125",null,"Lisovací kleště na konektory bez izolace 0,1-2,5mm2, paralelní lisování","1ks",161.43937116581495,{"$f":"F5396*(1-Elteq!$F$9)","v":161.43937116581495},"8591735023263"]
["TECHNIK","LK1-MO 0125 LOC",null,"Lisovací kleště s locatorem na konektory bez izolace 0,1-2,5mm2, paralelní lisování","1ks",193.72724539897791,{"$f":"F5397*(1-Elteq!$F$9)","v":193.72724539897791},"8591735048716"]
["TECHNIK","LK1-MO 056",null,"Lisovací kleště na konektory bez izolace 0,5-6mm2, paralelní lisování","1ks",158.47037123632867,{"$f":"F5398*(1-Elteq!$F$9)","v":158.47037123632867},"8591735023270"]
["TECHNIK","LK1-MO 056 LOC",null,"Lisovací kleště s locatorem na konektory bez izolace 0,5-6mm2, paralelní lisování","1ks",190.75824546949167,{"$f":"F5399*(1-Elteq!$F$9)","v":190.75824546949167},"8591735048723"]
["TECHNIK","LK-MO 0221",null,"Lisovací kleště na konektory bez izolace 0,2-2,1mm2, profi","1ks",77.193998166642544,{"$f":"F5400*(1-Elteq!$F$9)","v":77.193998166642544},"8591735008093"]
["TECHNIK","LK-MO 051 BP-A",null,"Lisovací kleště na konektory s bočním připojením typu A, průřez 0,5-1mm2","1ks",24.123124427075794,{"$f":"F5401*(1-Elteq!$F$9)","v":24.123124427075794},"8591735023355"]
["TECHNIK","LK-MO 051 BP-A/P",null,"Lisovací kleště na konektory s bočním připojením typu A, průřez 0,5-1mm2, rozměr 6,3x0,8mm","1ks",68.658123369369576,{"$f":"F5402*(1-Elteq!$F$9)","v":68.658123369369576},"8591735050948"]
["TECHNIK","LK-MO 0525",null,"Lisovací kleště na konektory bez izolace 0,5-2,5mm2 / 4,8mm + 6,3mm, economy","1ks",24.123124427075794,{"$f":"F5403*(1-Elteq!$F$9)","v":24.123124427075794},"8591735041557"]
["TECHNIK","LK-MO 0525 BP/P",null,"Lisovací kleště na konektory s bočním připojením typu A, průřez 0,5-2,5mm2","1ks",68.658123369369576,{"$f":"F5404*(1-Elteq!$F$9)","v":68.658123369369576},"8591735041755"]
["TECHNIK","LK-MO 0525 BP-B",null,"Lisovací kleště na konektory s bočním připojením typu B, průřez 0,5-2,5mm2","1ks",24.123124427075794,{"$f":"F5405*(1-Elteq!$F$9)","v":24.123124427075794},"8591735023362"]
["TECHNIK","LK-MO 0525 BP-B/P",null,"Lisovací kleště na konektory s bočním připojením typu B, průřez 0,5-2,5mm2, profi","1ks",68.658123369369576,{"$f":"F5406*(1-Elteq!$F$9)","v":68.658123369369576},"8591735050962"]
["TECHNIK","LK-MO 056",null,"Lisovací kleště na konektory bez izolace 0,5-6mm2 / 6,3mm, economy","1ks",24.123124427075794,{"$f":"F5407*(1-Elteq!$F$9)","v":24.123124427075794},"8591735008109"]
["TECHNIK","LK-MO 1525 BP-A",null,"Lisovací kleště na konektory s bočním připojením typu A, průřez 1,5-2,5mm2","1ks",24.123124427075794,{"$f":"F5408*(1-Elteq!$F$9)","v":24.123124427075794},"8591735023379"]
["TECHNIK","LK-MO 1525 BP-A/P",null,"Lisovací kleště na konektory s bočním připojením typu A, průřez 1,5-2,5mm2, rozměr 6,3x0,8mm","1ks",68.658123369369576,{"$f":"F5409*(1-Elteq!$F$9)","v":68.658123369369576},"8591735050955"]
["TECHNIK","LKR 0125",null,"975234 KNIPEX lisovací kleště na konektory bez izolace pro průřezy 0,1-2,5mm2","1ks",109.48187239980552,{"$f":"F5410*(1-Elteq!$F$9)","v":109.48187239980552},"8591735032944"]
["TECHNIK","LKR 056",null,"975235 KNIPEX lisovací kleště na konektory bez izolace pro průřezy 0,5-6mm2","1ks",109.48187239980552,{"$f":"F5411*(1-Elteq!$F$9)","v":109.48187239980552},"8591735032951"]
["TECHNIK","LKZ-MO 011",null,"Lisovací kleště na konektory bez izolace šíře 2,8mm pro průřezy 0,1-1mm2, zahnuté (LKF0,1-1)","1ks",26.720999365376265,{"$f":"F5412*(1-Elteq!$F$9)","v":26.720999365376265},"8591735049133"]
["TECHNIK","LKZ-MO 01425",null,"Lisovací kleště na konektory bez izolace šíře 2,8 a 4,8mm pro průřezy 0,14-2,5mm2 (LKF0,14-2,5)","1ks",26.720999365376265,{"$f":"F5413*(1-Elteq!$F$9)","v":26.720999365376265},"8591735049140"]
["TECHNIK","LKZ-MO 0256",null,"Lisovací kleště na konektory bez izolace šíře 6,3mm pro průřezy 0,25-6mm2, zahnuté (LKF0,25-6)","1ks",26.720999365376265,{"$f":"F5414*(1-Elteq!$F$9)","v":26.720999365376265},"8591735049157"]
["TECHNIK","LKZ-MO 051 BP-A",null,"Lisovací kleště na konektory s bočním připojením typu A, průřez 0,5-1mm2, zahnuté (LKBF0,5-1)","1ks",26.720999365376265,{"$f":"F5415*(1-Elteq!$F$9)","v":26.720999365376265},"8591735049195"]
["TECHNIK","LKZ-MO 0525 BP-B",null,"Lisovací kleště na konektory s bočním připojením typu B, průřez 0,5-2,5mm2, zahnuté (LKBF0,5-2,5)","1ks",26.720999365376265,{"$f":"F5416*(1-Elteq!$F$9)","v":26.720999365376265},"8591735049218"]
["TECHNIK","LKZ-MO 056",null,"Lisovací kleště na konektory bez izolace šíře 6,3mm pro průřezy 0,5-6mm2, zahnuté (LKF0,5-6)","1ks",24.494249418261575,{"$f":"F5417*(1-Elteq!$F$9)","v":24.494249418261575},"8591735049164"]
["TECHNIK","LKZ-MO 1525 BP-A",null,"Lisovací kleště na konektory s bočním připojením typu A, průřez 1,5-2,5mm2, zahnuté (LKBF1,5-2,5)","1ks",26.720999365376265,{"$f":"F5418*(1-Elteq!$F$9)","v":26.720999365376265},"8591735049201"]
["TECHNIK","CRIMPIT IT6L",null,"Lisovací kleště na izolované koncovky pro průřezy 0,5-6mm2, pevné čelisti","1ks",77.936248149014105,{"$f":"F5419*(1-Elteq!$F$9)","v":77.936248149014105},"8591735017637"]
["TECHNIK","CRIMPIT IT6S",null,"Lisovací kleště na izolované koncovky pro průřezy 0,5-6mm2, velmi robustní (CTI6)","1ks",162.73830863496516,{"$f":"F5420*(1-Elteq!$F$9)","v":162.73830863496516},"8591735017606"]
["TECHNIK","HNN 3",null,"Lisovací kleště na koncovky s izolací nylon 1,5-10mm2, crimpstar","1ks",78.307373140199886,{"$f":"F5421*(1-Elteq!$F$9)","v":78.307373140199886},"8591735007966"]
["TECHNIK","HNN 4",null,"Lisovací kleště na koncovky s izolací nylon 10-16mm2, crimpstar","1ks",78.307373140199886,{"$f":"F5422*(1-Elteq!$F$9)","v":78.307373140199886},"8591735007973"]
["TECHNIK","HP 1 crimpstar",null,"Lisovací kleště na izolované koncovky pro průřezy 0,20-2,5mm2, crimpstar","1ks",190.20155798271298,{"$f":"F5423*(1-Elteq!$F$9)","v":190.20155798271298},"8591735007980"]
["TECHNIK","HP 1/Z",null,"Lisovací kleště na izolované koncovky pro průřezy 0,1-1,5mm2, zahnuté","1ks",136.57399675636756,{"$f":"F5424*(1-Elteq!$F$9)","v":136.57399675636756},"8591735017675"]
["TECHNIK","HP 2/Z",null,"Lisovací kleště na izolované koncovky pro průřezy 0,5-2,5mm2, zahnuté","1ks",116.53324723233538,{"$f":"F5425*(1-Elteq!$F$9)","v":116.53324723233538},"8591735017682"]
["TECHNIK","HP 3",null,"Lisovací kleště na izolované koncovky pro průřezy 0,5-6mm2, profi","1ks",44.534998942293775,{"$f":"F5426*(1-Elteq!$F$9)","v":44.534998942293775},"8591735007997"]
["TECHNIK","HP 3 crimpstar",null,"Lisovací kleště na izolované koncovky pro průřezy 0,5-6mm2, crimpstar","1ks",77.936248149014105,{"$f":"F5427*(1-Elteq!$F$9)","v":77.936248149014105},"8591735036768"]
["TECHNIK","HP 3/TF",null,"Lisovací kleště na izolované koncovky pro průřezy 0,5-6mm2, robustní","1ks",68.658123369369576,{"$f":"F5428*(1-Elteq!$F$9)","v":68.658123369369576},"8591735023164"]
["TECHNIK","HP 3/Y",null,"Lisovací kleště na izolované koncovky pro průřezy 0,5-6mm2, stabilní","1ks",45.277248924665336,{"$f":"F5429*(1-Elteq!$F$9)","v":45.277248924665336},"8591735023171"]
["TECHNIK","KY 8161",null,"Lisovací kleště na izolované koncovky pro průřezy 0,5-6 mm2, paralelní chod čelistí","1ks",61.421186041246834,{"$f":"F5430*(1-Elteq!$F$9)","v":61.421186041246834},"8591735014513"]
["TECHNIK","KY-OI 056",null,"Lisovací kleště na izolované koncovky pro průřezy 0,5-6mm2, delší rukojeti","1ks",57.524373633796124,{"$f":"F5431*(1-Elteq!$F$9)","v":57.524373633796124},"8591735014506"]
["TECHNIK","LI 0,08-1,5",null,"Lisovací kleště na izolované koncovky pro průřezy 0,08-1,5mm2, zahnuté","1ks",21.525249488775323,{"$f":"F5432*(1-Elteq!$F$9)","v":21.525249488775323},"8591735023188"]
["TECHNIK","LI 0,25-2,5",null,"Lisovací kleště na izolované koncovky pro průřezy 0,25-2,5mm2, zahnuté","1ks",21.525249488775323,{"$f":"F5433*(1-Elteq!$F$9)","v":21.525249488775323},"8591735023195"]
["TECHNIK","LIR 056",null,"975236 KNIPEX lisovací kleště na izolované koncovky pro průřezy 0,5-6mm2","1ks",97.605872681860518,{"$f":"F5434*(1-Elteq!$F$9)","v":97.605872681860518},"8591735033453"]
["TECHNIK","LK-0525 BP",null,"Lisovací kleště na izolované konektory s bočním připojením pro průřezy 0,5-2,5mm2, economy","1ks",27.83437433893361,{"$f":"F5435*(1-Elteq!$F$9)","v":27.83437433893361},"8591735023201"]
["TECHNIK","LK-0525 BP/P",null,"Lisovací kleště na izolované konektory s bočním připojením pro průřezy 0,5-2,5mm2, profi","1ks",59.008873598539253,{"$f":"F5436*(1-Elteq!$F$9)","v":59.008873598539253},"8591735041793"]
["TECHNIK","LK1-OI 056",null,"Lisovací kleště na izolované koncovky pro průřezy 0,5-6mm2, paralelní lisování","1ks",145.10987155364055,{"$f":"F5437*(1-Elteq!$F$9)","v":145.10987155364055},"8591735017590"]
["TECHNIK","LK1-OI 1016",null,"Lisovací kleště na izolované koncovky pro průřezy 10-16mm2, paralelní lisování","1ks",148.07887148312679,{"$f":"F5438*(1-Elteq!$F$9)","v":148.07887148312679},"8591735023287"]
["TECHNIK","LK1-SIS 056",null,"Lisovací kleště na koncovky se smrštitelnou bužírkou pro průřezy 0,5-6mm2, paralelní lisování","1ks",145.10987155364055,{"$f":"F5439*(1-Elteq!$F$9)","v":145.10987155364055},"8591735048709"]
["TECHNIK","LK-OI 056",null,"Lisovací kleště na izolované koncovky pro průřezy 0,5-6mm2, economy","1ks",24.123124427075794,{"$f":"F5440*(1-Elteq!$F$9)","v":24.123124427075794},"8591735002046"]
["TECHNIK","LKZ-0525 BP",null,"Lisovací kleště na izolované konektory s bočním připojením 0,5-2,5mm2, zahnuté (LIBF0,5-45)","1ks",26.720999365376265,{"$f":"F5441*(1-Elteq!$F$9)","v":26.720999365376265},"8591735049126"]
["TECHNIK","LKZ-OI 0146",null,"Lisovací kleště na izolované koncovky pro průřezy 0,14-6mm2, zahnuté (LIF0,14-6)","1ks",24.494249418261575,{"$f":"F5442*(1-Elteq!$F$9)","v":24.494249418261575},"8591735049096"]
["TECHNIK","LKZ-OI 056",null,"Lisovací kleště na izolované koncovky pro průřezy 0,5-6mm2, zahnuté (LIF0,5-6)","1ks",24.494249418261575,{"$f":"F5443*(1-Elteq!$F$9)","v":24.494249418261575},"8591735049102"]
["TECHNIK","LKZ-OI 1016",null,"Lisovací kleště na izolované koncovky pro průřezy 10-16mm2, zahnuté (LIF10-16)","1ks",24.494249418261575,{"$f":"F5444*(1-Elteq!$F$9)","v":24.494249418261575},"8591735049119"]
["TECHNIK","HN 1",null,"Lisovací kleště na oka neizolovaná pro průřezy 0,5-10mm2, profi","1ks",44.534998942293775,{"$f":"F5445*(1-Elteq!$F$9)","v":44.534998942293775},"8591735007942"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"HN 1 crimpstar",null,"Lisovací kleště na oka neizolovaná pro průřezy 0,5-10mm2, crimpstar","1ks",65.689123439883318,{"$f":"F5446*(1-Elteq!$F$9)","v":65.689123439883318},""]
["TECHNIK","HN 1/TF",null,"Lisovací kleště na oka neizolovaná pro průřezy 0,5-10mm2, robustní","1ks",68.658123369369576,{"$f":"F5447*(1-Elteq!$F$9)","v":68.658123369369576},"8591735023133"]
["TECHNIK","HN 1/Y",null,"Lisovací kleště na oka neizolovaná pro průřezy 0,5-10mm2, pevné čelisti","1ks",45.462811420258227,{"$f":"F5448*(1-Elteq!$F$9)","v":45.462811420258227},"8591735023140"]
["TECHNIK","HN 5 crimpstar",null,"Lisovací kleště na oka neizolovaná pro průřezy 10-16mm2, crimpstar","1ks",65.689123439883318,{"$f":"F5449*(1-Elteq!$F$9)","v":65.689123439883318},"8591735007959"]
["TECHNIK","HN 5/Y",null,"Lisovací kleště na oka neizolovaná pro průřezy 10-16mm2, pevné čelisti","1ks",48.060686358558698,{"$f":"F5450*(1-Elteq!$F$9)","v":48.060686358558698},"8591735023157"]
["TECHNIK","HN 7",null,"Lisovací kleště na oka neizolovaná pro průřezy 10-25mm2, profi","1ks",57.524373633796124,{"$f":"F5451*(1-Elteq!$F$9)","v":57.524373633796124},"8591735035631"]
["TECHNIK","HN 7/TF",null,"Lisovací kleště na oka neizolovaná pro průřezy 10-25mm2, robustní","1ks",92.038997814073795,{"$f":"F5452*(1-Elteq!$F$9)","v":92.038997814073795},"8591735041489"]
["TECHNIK","HP4-C10",null,"Lisovací kleště na Cu odbočné svorky C6 - C10","1ks",318.79636742858628,{"$f":"F5453*(1-Elteq!$F$9)","v":318.79636742858628},"8591735033200"]
["TECHNIK","KY-ON 0510",null,"Lisovací kleště na neizolovaná oka a spojky pro průřezy 0,5-10mm2, delší rukojeti","1ks",57.524373633796124,{"$f":"F5454*(1-Elteq!$F$9)","v":57.524373633796124},"8591735037772"]
["TECHNIK","LK1-OL 1510",null,"Lisovací kleště na oka lehčená pro průřezy 1,5-10mm2, paralelní lisování","1ks",143.62537158889742,{"$f":"F5455*(1-Elteq!$F$9)","v":143.62537158889742},"8591735023317"]
["TECHNIK","LK1-ON 02525",null,"Lisovací kleště na oka neizolovaná pro průřezy 0,25-2,5mm2, paralelní lisování","1ks",144.73874656245476,{"$f":"F5456*(1-Elteq!$F$9)","v":144.73874656245476},"8591735023294"]
["TECHNIK","LK1-ON 0510",null,"Lisovací kleště na oka neizolovaná pro průřezy 0,5-10mm2, paralelní lisování","1ks",143.62537158889742,{"$f":"F5457*(1-Elteq!$F$9)","v":143.62537158889742},"8591735023300"]
["TECHNIK","LK1-ON 1625",null,"Lisovací kleště na oka neizolovaná pro průřezy 16-25mm2, paralelní lisování","1ks",146.59437151838367,{"$f":"F5458*(1-Elteq!$F$9)","v":146.59437151838367},"8591735023324"]
["TECHNIK","LK-KK 02515",null,"Lisovací kleště na kruhové konektory 0,25-1,5mm2, economy","1ks",36.741374127392362,{"$f":"F5459*(1-Elteq!$F$9)","v":36.741374127392362},"8591735008062"]
["TECHNIK","LK-KK 02515/P",null,"Lisovací kleště na kruhové konektory 0,25-1,5mm2, profi","1ks",53.813123721938311,{"$f":"F5460*(1-Elteq!$F$9)","v":53.813123721938311},"8591735041786"]
["TECHNIK","LK-OL 056",null,"Lisovací kleště na oka lehčená pro průřezy 0,5-6mm2 šestihran, economy","1ks",61.606748536839724,{"$f":"F5461*(1-Elteq!$F$9)","v":61.606748536839724},"8591735041748"]
["TECHNIK","LK-OL 056/P",null,"Lisovací kleště na oka lehčená pro průřezy 0,5-6mm2 šestihran, profi","1ks",68.658123369369576,{"$f":"F5462*(1-Elteq!$F$9)","v":68.658123369369576},"8591735041731"]
["TECHNIK","LK-OL 07516",null,"Lisovací kleště na oka lehčená pro průřezy 0,75-16mm2, profi (K2)","1ks",148.11598398224538,{"$f":"F5463*(1-Elteq!$F$9)","v":148.11598398224538},"8591735008123"]
["TECHNIK","LK-ON 0510",null,"Lisovací kleště na oka neizolovaná pro průřezy 0,5-10mm2, economy","1ks",24.123124427075794,{"$f":"F5464*(1-Elteq!$F$9)","v":24.123124427075794},"8591735008147"]
["TECHNIK","LK-ON 0516",null,"Lisovací kleště na oka neizolovaná pro průřezy 0,5-16mm2, profi (K25)","1ks",148.11598398224538,{"$f":"F5465*(1-Elteq!$F$9)","v":148.11598398224538},"8591735008130"]
["TECHNIK","LKZ-ON 0510",null,"Lisovací kleště na oka a spojky bez izolace pro průřezy 0,5-10mm2, zahnuté (LNF1,5-10)","1ks",24.494249418261575,{"$f":"F5466*(1-Elteq!$F$9)","v":24.494249418261575},"8591735049171"]
["TECHNIK","LKZ-ON 2516",null,"Lisovací kleště na oka a spojky bez izolace pro průřezy 2,5-16mm2, zahnuté (LNF2,5-16)","1ks",24.494249418261575,{"$f":"F5467*(1-Elteq!$F$9)","v":24.494249418261575},"8591735049188"]
["TECHNIK","LN 0,25-2,5",null,"Lisovací kleště na neizolované koncovky 0,25-2,5mm2, zahnuté","1ks",21.525249488775323,{"$f":"F5468*(1-Elteq!$F$9)","v":21.525249488775323},"8591735023386"]
["TECHNIK","LN 1,5-6",null,"Lisovací kleště na oka neizolovaná pro průřezy 1,5-6mm2, zahnuté","1ks",21.525249488775323,{"$f":"F5469*(1-Elteq!$F$9)","v":21.525249488775323},"8591735023393"]
["TECHNIK","LNR 02525",null,"Lisovací kleště na oka neizolovaná 0,25-2,5mm2, kvalitní Knipex","1ks",95.379122734745835,{"$f":"F5470*(1-Elteq!$F$9)","v":95.379122734745835},""]
["TECHNIK","LNR 0510",null,"975233 KNIPEX lisovací kleště na oka neizolovaná pro průřezy 0,5-10mm2","1ks",95.379122734745835,{"$f":"F5471*(1-Elteq!$F$9)","v":95.379122734745835},""]
["TECHNIK","LSR 1510",null,"975230 KNIPEX lisovací kleště na Cu odlehčené spojky pro průřezy 1,5-10mm2","1ks",95.750247725931615,{"$f":"F5472*(1-Elteq!$F$9)","v":95.750247725931615},"8591735033316"]
["TECHNIK","NK 13",null,"Napínací kleště na plastové vázací pásky do šíře 13,5mm economy","1ks",29.504436799269627,{"$f":"F5473*(1-Elteq!$F$9)","v":29.504436799269627},"8591735008734"]
["TECHNIK","NK 13 H - MK9",null,"Napínací kleště na plastové vázací pásky do šíře 13,5mm HELLERMANN","1ks",342.3256918697648,{"$f":"F5474*(1-Elteq!$F$9)","v":342.3256918697648},"8591735041441"]
["TECHNIK","NK 46",null,"Napínací kleště na plastové vázací pásky do šíře 4,8mm standard","1ks",63.685048487480096,{"$f":"F5475*(1-Elteq!$F$9)","v":63.685048487480096},"8591735041458"]
["TECHNIK","NK 48",null,"Napínací kleště na plastové vázací pásky do šíře 4,8mm economy","1ks",24.494249418261575,{"$f":"F5476*(1-Elteq!$F$9)","v":24.494249418261575},"8591735008741"]
["TECHNIK","NK 48 H - EVO7",null,"Napínací kleště na plastové vázací pásky do šíře 4,8mm HELLERMANN novinka","1ks",344.10709182745654,{"$f":"F5477*(1-Elteq!$F$9)","v":344.10709182745654},""]
["TECHNIK","NK 48 P - GS2B",null,"Napínací kleště na plastové vázací pásky do šíře 4,8mm PANDUIT","1ks",238.07668184567879,{"$f":"F5478*(1-Elteq!$F$9)","v":238.07668184567879},""]
["TECHNIK","NK 48 P - GTS",null,"Napínací kleště na plastové vázací pásky do šíře 4,8mm PANDUIT","1ks",220.63380725994708,{"$f":"F5479*(1-Elteq!$F$9)","v":220.63380725994708},"8591735041502"]
["TECHNIK","NK 9",null,"Napínací kleště na plastové pásky do šíře 9,0mm s integrovaným střihacím mechanismem","1ks",20.411874515217981,{"$f":"F5480*(1-Elteq!$F$9)","v":20.411874515217981},"8591735055790"]
["TECHNIK","NK 9 P - GTH",null,"Napínací kleště na plastové vázací pásky do šíře 9,0mm PANDUIT","1ks",275.37474345984987,{"$f":"F5481*(1-Elteq!$F$9)","v":275.37474345984987},"8591735041496"]
["TECHNIK","NKST 12",null,"Napínací kleště na kovové vázací pásky do šíře 12mm profi","1ks",162.92387113055807,{"$f":"F5482*(1-Elteq!$F$9)","v":162.92387113055807},"8591735016456"]
["TECHNIK","NKST 8",null,"Napínací kleště na kovové vázací pásky do šíře 7,9mm a síly 0,3mm profi","1ks",81.647498060871925,{"$f":"F5483*(1-Elteq!$F$9)","v":81.647498060871925},"8591735016449"]
["TECHNIK","PTS 48",null,"Napínací kleště na plastové vázací pásky do šíře 4,8mm pneumatické PANDUIT","1ks",1015.2124133887052,{"$f":"F5484*(1-Elteq!$F$9)","v":1015.2124133887052},"8591735042073"]
["TECHNIK","VS-hlavička",null,"Náhradní hlavička","1ks",14.956337144786993,{"$f":"F5485*(1-Elteq!$F$9)","v":14.956337144786993},"8591735009922"]
["TECHNIK","VS-komplet",null,"Vázací souprava komplet pro pásku šíře 4,5mm s nosností 25kg","1ks",68.658123369369576,{"$f":"F5486*(1-Elteq!$F$9)","v":68.658123369369576},"8591735008758"]
["TECHNIK","VS-nůž",null,"Náhradní nůž","1ks",6.4946873457511751,{"$f":"F5487*(1-Elteq!$F$9)","v":6.4946873457511751},"8591735009939"]
["TECHNIK","VS-páska bílá",null,"Vázací páska bílá 15m role","15m",26.720999365376265,{"$f":"F5488*(1-Elteq!$F$9)","v":26.720999365376265},"8591735008765"]
["TECHNIK","VS-páska černá",null,"Vázací páska černá UV odolná 15m role","15m",26.720999365376265,{"$f":"F5489*(1-Elteq!$F$9)","v":26.720999365376265},"8591735008772"]
["TECHNIK","VS-spona bílá",null,"Vázací spona bílá 200ks","200ks",22.638624462332668,{"$f":"F5490*(1-Elteq!$F$9)","v":22.638624462332668},"8591735008789"]
["TECHNIK","VS-spona černá",null,"Vázací spona černá UV odolná 200ks","200ks",22.638624462332668,{"$f":"F5491*(1-Elteq!$F$9)","v":22.638624462332668},"8591735008796"]
["TECHNIK","BZ 44F",null,"Nýtovací kleště pro nýty Al, Cu 3-5mm / Fe 3-4mm","1ks",55.186286189325706,{"$f":"F5492*(1-Elteq!$F$9)","v":55.186286189325706},"8591735014643"]
["TECHNIK","BZ 44F pružina",null,"Náhradní pružina do kleští BZ 44F","1ks",4.5648373915851117,{"$f":"F5493*(1-Elteq!$F$9)","v":4.5648373915851117},""]
["TECHNIK","HN 2",null,"Nýtovací kleště pro nýty 4-6,4mm","1ks",268.06358113348995,{"$f":"F5494*(1-Elteq!$F$9)","v":268.06358113348995},""]
["TECHNIK","HN 35",null,"Nýtovací kleště pro nýty Al, Cu 3-5mm / Fe 3-4mm","1ks",37.743411603593977,{"$f":"F5495*(1-Elteq!$F$9)","v":37.743411603593977},"8591735013073"]
["TECHNIK","KL 01",null,"Náhradní kleštiny pro kleště HN 35, BZ 44F, S","1ks",17.888224575154666,{"$f":"F5496*(1-Elteq!$F$9)","v":17.888224575154666},""]
["TECHNIK","S",null,"Nýtovací kleště pro nýty Al, Cu 3-5mm / Fe 3-4mm","1ks",58.786198603827785,{"$f":"F5497*(1-Elteq!$F$9)","v":58.786198603827785},"8591735013080"]
["TECHNIK","SN 2",null,"Nýtovací kleště pro nýty 4-6,4mm","1ks",312.11611758724223,{"$f":"F5498*(1-Elteq!$F$9)","v":312.11611758724223},""]
["TECHNIK","45-120",null,"Odizolovací kleště IDEAL T®-5 T®-Stripper Wire Stripper, Solid 10-18, Stranded 12-20","1ks",52.068836263365135,{"$f":"F5499*(1-Elteq!$F$9)","v":52.068836263365135},""]
["TECHNIK","45-120-341",null,"Odizolovací kleště IDEAL T®-Stripper Wire Stripper, Metric 0,75-6mm2","1ks",52.068836263365135,{"$f":"F5500*(1-Elteq!$F$9)","v":52.068836263365135},""]
["TECHNIK","45-121",null,"Odizolovací kleště IDEAL T®-6 T®-Stripper Wire Stripper, Solid 14-24, Stranded 16-26","1ks",52.068836263365135,{"$f":"F5501*(1-Elteq!$F$9)","v":52.068836263365135},""]
["TECHNIK","45-125",null,"Odizolovací kleště IDEAL T®-7 T®-Stripper Wire Stripper, Solid 22-30, Stranded 24-32","1ks",52.068836263365135,{"$f":"F5502*(1-Elteq!$F$9)","v":52.068836263365135},""]
["TECHNIK","45-125-341",null,"Odizolovací kleště IDEAL T®-Stripper Wire Stripper, Metric 0,5-4mm2","1ks",52.068836263365135,{"$f":"F5503*(1-Elteq!$F$9)","v":52.068836263365135},""]
["TECHNIK","C-SCORA  2T",null,"Náhradní odizolovací břity 0,03-2,08mm2 do kleští SCORA 2T","1sada",50.101873810080498,{"$f":"F5504*(1-Elteq!$F$9)","v":50.101873810080498},""]
["TECHNIK","C-SCORA  6T",null,"Náhradní odizolovací břity 0,14-6mm2 do kleští SCORA 6T","1sada",50.101873810080498,{"$f":"F5505*(1-Elteq!$F$9)","v":50.101873810080498},""]
["TECHNIK","C-SCORA 10T",null,"Náhradní odizolovací břity 2,5-10mm2 do kleští SCORA 10T","1sada",50.101873810080498,{"$f":"F5506*(1-Elteq!$F$9)","v":50.101873810080498},"8591735038588"]
["TECHNIK","C-SCORA 16T",null,"Náhradní odizolovací břity 16mm2 do kleští SCORA 16T","1sada",50.101873810080498,{"$f":"F5507*(1-Elteq!$F$9)","v":50.101873810080498},""]
["TECHNIK","C-SCORA 25T",null,"Náhradní odizolovací břity 25mm2 do kleští SCORA 25T","1sada",50.101873810080498,{"$f":"F5508*(1-Elteq!$F$9)","v":50.101873810080498},""]
["TECHNIK","C-SCORA 2x1/4,8/6,6",null,"Náhradní odizolovací břity s průměry 2x1,0mm / 4,8mm / 6,6mm do kleští SCORA T","1sada",50.101873810080498,{"$f":"F5509*(1-Elteq!$F$9)","v":50.101873810080498},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"C-SCORA 6Tsolar",null,"Náhradní odizolovací břity 1,5-6mm2 do kleští SCORA 6T solar","1sada",50.101873810080498,{"$f":"F5510*(1-Elteq!$F$9)","v":50.101873810080498},""]
["TECHNIK","C-SCORA 708216",null,"Náhradní odizolovací břity 708216 do kleští SCORA","1sada",50.101873810080498,{"$f":"F5511*(1-Elteq!$F$9)","v":50.101873810080498},""]
["TECHNIK","C-SCORA 708245",null,"Náhradní odizolovací břity 708245 do kleští SCORA","1sada",50.101873810080498,{"$f":"F5512*(1-Elteq!$F$9)","v":50.101873810080498},""]
["TECHNIK","C-SCORA 8,9",null,"Náhradní odizolovací břity s průměrem 8,9mm do kleští SCORA T","1sada",50.101873810080498,{"$f":"F5513*(1-Elteq!$F$9)","v":50.101873810080498},""]
["TECHNIK","ECOSTRIP 6",null,"Odizolovací kleště pro průřezy 0,2-6mm2","1ks",21.154124497589542,{"$f":"F5514*(1-Elteq!$F$9)","v":21.154124497589542},"8591735012816"]
["TECHNIK","JOKARI  6",null,"1262180 KNIPEX odizolovací kleště pro průřezy 0,2-6mm2 se silnější konstrukcí JOKARI","1ks",29.578661797506783,{"$f":"F5515*(1-Elteq!$F$9)","v":29.578661797506783},"8591735036690"]
["TECHNIK","JOKARI  6N",null,"Odizolovací kleště pro průřezy 0,2-6mm2 super 4 plus JOKARI 100780","1ks",19.298499541660636,{"$f":"F5516*(1-Elteq!$F$9)","v":19.298499541660636},"8591735054625"]
["TECHNIK","JOKARI 16",null,"Odizolovací kleště pro průřezy 6-16mm2 JOKARI","1ks",69.511710849096872,{"$f":"F5517*(1-Elteq!$F$9)","v":69.511710849096872},""]
["TECHNIK","SCORA  2",null,"1211180 KNIPEX odizolovací kleště profesionální pro průřezy 0,5-2mm2","1ks",56.63367365495025,{"$f":"F5518*(1-Elteq!$F$9)","v":56.63367365495025},"8591735022471"]
["TECHNIK","SCORA  2T",null,"121202 KNIPEX odizolovací kleště profesionální pro průřezy 0,03-2,08mm2","1ks",103.54387254083302,{"$f":"F5519*(1-Elteq!$F$9)","v":103.54387254083302},"8591735019570"]
["TECHNIK","SCORA  6",null,"1221180 KNIPEX odizolovací kleště profesionální pro průřezy 0,5-6mm2","1ks",57.78416112762617,{"$f":"F5520*(1-Elteq!$F$9)","v":57.78416112762617},"8591735008369"]
["TECHNIK","SCORA  6T",null,"121206 KNIPEX odizolovací kleště profi pro průřezy 0,14-6mm2, ostří 0,7/1,35/1,7/2,3/2,7/3,5mm","1ks",103.54387254083302,{"$f":"F5521*(1-Elteq!$F$9)","v":103.54387254083302},"8591735019587"]
["TECHNIK","SCORA  6Tsolar",null,"121211 KNIPEX dizolovací kleště profesionální pro průřezy 1,5-6mm2 na solární kabely","1ks",103.54387254083302,{"$f":"F5522*(1-Elteq!$F$9)","v":103.54387254083302},"8591735030568"]
["TECHNIK","SCORA  D",null,"Odizolovací kleště profesionální na dvoulinku pro průřezy 2x1,5mm2","1ks",103.54387254083302,{"$f":"F5523*(1-Elteq!$F$9)","v":103.54387254083302},""]
["TECHNIK","SCORA 10",null,"1240200 KNIPEX odizolovací kleště profesionální pro průřezy 0,03-10mm2","1ks",67.17362340462644,{"$f":"F5524*(1-Elteq!$F$9)","v":67.17362340462644},"8591735010690"]
["TECHNIK","SCORA 10P",null,"1242195 KNIPEX odizolovací kleště profesionální 0,03-10mm2 MULTISTRIP","1ks",86.100997955101292,{"$f":"F5525*(1-Elteq!$F$9)","v":86.100997955101292},"8591735019617"]
["TECHNIK","SCORA 10T",null,"121210 KNIPEX odizolovací kleště profi pro průřezy 2,5-10mm2, průměr ostří 2,3/2,7/3,5/4,45mm","1ks",103.54387254083302,{"$f":"F5526*(1-Elteq!$F$9)","v":103.54387254083302},"8591735019594"]
["TECHNIK","SCORA 16",null,"1250200 KNIPEX odizolovací kleště profesionální pro průřezy 2,5-16mm2","1ks",99.090372646603655,{"$f":"F5527*(1-Elteq!$F$9)","v":99.090372646603655},"8591735011659"]
["TECHNIK","SCORA 16T",null,"Odizolovací kleště profesionální pro průřezy 16mm2 (na zakázku 6-16mm2, ostří 3,5/4,45/5,7mm)","1ks",103.54387254083302,{"$f":"F5528*(1-Elteq!$F$9)","v":103.54387254083302},"8591735036805"]
["TECHNIK","SCORA 25T",null,"Odizolovací kleště profesionální pro průřez 25mm2, průměr ostří 7,3mm","1ks",103.54387254083302,{"$f":"F5529*(1-Elteq!$F$9)","v":103.54387254083302},"8591735036812"]
["TECHNIK","SCORA 35T",null,"Odizolovací kleště profesionální pro průřez 35mm2, průměr ostří 8,5mm","1ks",103.54387254083302,{"$f":"F5530*(1-Elteq!$F$9)","v":103.54387254083302},"8591735055561"]
["TECHNIK","SCORA AWG 16-26",null,"121214 KNIPEX odizolovací kleště profi pro průřezy AWG 16-26, prům. ostří 0,3/0,55/0,8/1,1/1,4/1,6mm","1ks",103.54387254083302,{"$f":"F5531*(1-Elteq!$F$9)","v":103.54387254083302},"8591735056032"]
["TECHNIK","SCORA T",null,"Odizolovací kleště profesionální bez čelistí","1ks",54.555373704309872,{"$f":"F5532*(1-Elteq!$F$9)","v":54.555373704309872},"8591735030681"]
["TECHNIK","STRIPAX 1",null,"1260135 KNIPEX odizolovací kleště automatické 0,02-1mm2 profi Weidmüller 9001280000","1ks",65.689123439883318,{"$f":"F5533*(1-Elteq!$F$9)","v":65.689123439883318},"8591735036447"]
["TECHNIK","STRIPAX 10",null,"Odizolovací kleště automatické 0,08-10mm2, profesionální Weidmüller 9005000000","1ks",67.17362340462644,{"$f":"F5534*(1-Elteq!$F$9)","v":67.17362340462644},"8591735054632"]
["TECHNIK","STRIPAX 16",null,"Odizolovací kleště automatické 6-16mm2, profesionální Weidmüller 9005610000","1ks",105.77062248794772,{"$f":"F5535*(1-Elteq!$F$9)","v":105.77062248794772},"8591735054649"]
["TECHNIK","STRIPAX 6",null,"Odizolovací kleště automatické 0,08-6mm2, profesionální provedení","1ks",66.431373422254879,{"$f":"F5536*(1-Elteq!$F$9)","v":66.431373422254879},"8591735008376"]
["TECHNIK","STRIPAX 6H",null,"Odizolovací kleště automatické 0,08-6mm2, ekonomické provedení","1ks",36.741374127392362,{"$f":"F5537*(1-Elteq!$F$9)","v":36.741374127392362},"8591735041922"]
["TECHNIK","STRIPAX 6UL",null,"Odizolovací kleště automatické 0,14-6mm2, profesionální Weidmüller ultimate 1468880000","1ks",76.266185688678092,{"$f":"F5538*(1-Elteq!$F$9)","v":76.266185688678092},"8591735054656"]
["TECHNIK","STRIPIT 16",null,"Odizolovací kleště automatické 6-16mm2 profesionální (STRIPAX 16)","1ks",129.52262192383773,{"$f":"F5539*(1-Elteq!$F$9)","v":129.52262192383773},""]
["TECHNIK","STRIPIT 6",null,"Odizolovací kleště automatické 0,08-6mm2 profesionální (STRIPAX 6)","1ks",66.431373422254879,{"$f":"F5540*(1-Elteq!$F$9)","v":66.431373422254879},"8591735010683"]
["TECHNIK","WE 1,5",null,"Odizolovací kleště pro průřezy 0,08-1,5mm2 profesionální Micro Strip","1ks",35.999124145020801,{"$f":"F5541*(1-Elteq!$F$9)","v":35.999124145020801},"8591735050597"]
["TECHNIK","WE 25",null,"Odizolovací kleště pro průřezy 1,0-25mm2 profesionální Mega Strip","1ks",120.0589346486003,{"$f":"F5542*(1-Elteq!$F$9)","v":120.0589346486003},"8591735009526"]
["TECHNIK","WE 5",null,"Odizolovací kleště pro průřezy 0,2-6mm2 s funkcí stříhání vodičů do průměru 2mm","1ks",27.83437433893361,{"$f":"F5543*(1-Elteq!$F$9)","v":27.83437433893361},"8591735008888"]
["TECHNIK","WE 5/1000",null,"Odizolovací kleště pro průřezy 0,5-6mm2 izolované do 1000V (WE6KV)","1ks",35.25687416264924,{"$f":"F5544*(1-Elteq!$F$9)","v":35.25687416264924},"8591735038106"]
["TECHNIK","WE 7F",null,"Odizolovací kleště pro průřezy 0,75-4mm2 na ploché kabely","1ks",59.008873598539253,{"$f":"F5545*(1-Elteq!$F$9)","v":59.008873598539253},"8591735038113"]
["TECHNIK","WE 7R",null,"Odizolovací kleště pro průřezy 0,5-16mm2 na kruhové vodiče","1ks",59.008873598539253,{"$f":"F5546*(1-Elteq!$F$9)","v":59.008873598539253},"8591735038120"]
["TECHNIK","WE 7S",null,"Odizolovací kleště pro průřezy 1,5-6mm2 na solární kabely","1ks",59.008873598539253,{"$f":"F5547*(1-Elteq!$F$9)","v":59.008873598539253},"8591735038137"]
["TECHNIK","WE150",null,"Odizolovací kleště pro průřezy 0,5-6mm2 s funkcí stříhání do 6mm2 laněné, do 4mm2 plné vodiče","1ks",21.154124497589542,{"$f":"F5548*(1-Elteq!$F$9)","v":21.154124497589542},"8591735008901"]
["TECHNIK","WE200",null,"Odizolovací kleště pro vodiče o průměru 4-28mm a vnitřní vodiče o průřezu 0,5-6mm2","1ks",40.823749030435962,{"$f":"F5549*(1-Elteq!$F$9)","v":40.823749030435962},"8591735008925"]
["TECHNIK","KY 2",null,"Tříhroté roztahovací kleště na navlékání gumových trubiček 1,7-5mm / kabel max. 9mm (hroty 4,38mm)","1ks",66.431373422254879,{"$f":"F5550*(1-Elteq!$F$9)","v":66.431373422254879},"8591735054953"]
["TECHNIK","KY 3",null,"Tříhroté roztahovací kleště na navlékání gumových trubiček 3-10mm / kabel max. 15mm (hroty 5,68mm)","1ks",66.431373422254879,{"$f":"F5551*(1-Elteq!$F$9)","v":66.431373422254879},"8591735052324"]
["TECHNIK","KY 4",null,"Tříhroté roztahovací kleště na navlékání gumových trubiček 10-17mm / kabel max. 28mm (hroty 0,00mm)","1ks",66.431373422254879,{"$f":"F5552*(1-Elteq!$F$9)","v":66.431373422254879},"8591735056353"]
["TECHNIK","PB  8",null,"Olověná plomba velikost 8mm","100ks",6.6802498413440663,{"$f":"F5553*(1-Elteq!$F$9)","v":6.6802498413440663},""]
["TECHNIK","PB 10",null,"Olověná plomba velikost 10mm","100ks",7.4224998237156292,{"$f":"F5554*(1-Elteq!$F$9)","v":7.4224998237156292},""]
["TECHNIK","PB 12",null,"Olověná plomba velikost 12mm","100ks",10.205937257608991,{"$f":"F5555*(1-Elteq!$F$9)","v":10.205937257608991},"8591735055028"]
["TECHNIK","PB 14",null,"Olověná plomba velikost 14mm","100ks",11.875999717945007,{"$f":"F5556*(1-Elteq!$F$9)","v":11.875999717945007},""]
["TECHNIK","PBD 300",null,"Plombovací drát průměr 1,1mm sekaný na délku 300mm ČSN 15 3924","100ks",4.4534998942293775,{"$f":"F5557*(1-Elteq!$F$9)","v":4.4534998942293775},"8591735038625"]
["TECHNIK","PBK 10",null,"Plombovací kleště pro průměr plomby 10mm","1ks",59.008873598539253,{"$f":"F5558*(1-Elteq!$F$9)","v":59.008873598539253},""]
["TECHNIK","PBK 12",null,"Plombovací kleště pro průměr plomby 12mm","1ks",59.008873598539253,{"$f":"F5559*(1-Elteq!$F$9)","v":59.008873598539253},""]
["TECHNIK","PBK 14",null,"Plombovací kleště pro průměr plomby 14mm","1ks",59.008873598539253,{"$f":"F5560*(1-Elteq!$F$9)","v":59.008873598539253},""]
["TECHNIK","PBR  8",null,"Plombovací razidlo průměr 8mm","1ks",4.861737384533737,{"$f":"F5561*(1-Elteq!$F$9)","v":4.861737384533737},""]
["TECHNIK","PBR  9",null,"Plombovací razidlo průměr 9mm","1ks",4.861737384533737,{"$f":"F5562*(1-Elteq!$F$9)","v":4.861737384533737},""]
["TECHNIK","PBR 10",null,"Plombovací razidlo průměr 10mm","1ks",4.861737384533737,{"$f":"F5563*(1-Elteq!$F$9)","v":4.861737384533737},""]
["TECHNIK","PBR 14",null,"Plombovací razidlo průměr 14mm","1ks",4.861737384533737,{"$f":"F5564*(1-Elteq!$F$9)","v":4.861737384533737},""]
["TECHNIK","PPB  6",null,"Plastová plomba rudá velikost 6","100ks",2.8947749312490956,{"$f":"F5565*(1-Elteq!$F$9)","v":2.8947749312490956},"8591735038632"]
["TECHNIK","PPB  8",null,"Plastová plomba rudá velikost 8","100ks",2.8947749312490956,{"$f":"F5566*(1-Elteq!$F$9)","v":2.8947749312490956},"8591735038649"]
["TECHNIK","PPB 10",null,"Plastová plomba rudá velikost 11","100ks",2.8947749312490956,{"$f":"F5567*(1-Elteq!$F$9)","v":2.8947749312490956},"8591735038656"]
["TECHNIK","PPB 15",null,"Plastová plomba rudá velikost 15","100ks",3.3401249206720331,{"$f":"F5568*(1-Elteq!$F$9)","v":3.3401249206720331},"8591735038663"]
["TECHNIK","LKM 6/70",null,"Lisovací kleště s otočnými čelistmi na oka lehčená 6-70mm2, profi","1ks",226.75736961451247,{"$f":"F5569*(1-Elteq!$F$9)","v":226.75736961451247},"8591735008024"]
["TECHNIK","LKM 6/70 D",null,"Lisovací kleště s otočnými čelistmi na oka dle DIN 6-70mm2, profi","1ks",226.75736961451247,{"$f":"F5570*(1-Elteq!$F$9)","v":226.75736961451247},"8591735008031"]
["TECHNIK","MHP  6/50",null,"Lisovací kleště s otočnými čelistmi na standardní Cu oka lehčená 6-50mm2, profi K05","1ks",127.66699696790882,{"$f":"F5571*(1-Elteq!$F$9)","v":127.66699696790882},"8591735023409"]
["TECHNIK","MHP  6/50 D",null,"Lisovací kleště s otočnými čelistmi na oka Cu DIN 6-50mm2 a AL 10-35mm2, profi K05D","1ks",127.66699696790882,{"$f":"F5572*(1-Elteq!$F$9)","v":127.66699696790882},"8591735023416"]
["TECHNIK","MHP 10/120",null,"Lisovací kleště s otočnými čelistmi na standardní Cu oka lehčená 10-120mm2, profi K06","1ks",179.995620725104,{"$f":"F5573*(1-Elteq!$F$9)","v":179.995620725104},"8591735023423"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"MHP 10/120 D",null,"Lisovací kleště s otočnými čelistmi na oka Cu DIN 10-120mm2 a AL 10-95mm2, profi K06D","1ks",183.70687063696181,{"$f":"F5574*(1-Elteq!$F$9)","v":183.70687063696181},"8591735017279"]
["TECHNIK","MHP 16/95",null,"Lisovací kleště s otočnými čelistmi na standardní Cu oka lehčená 16-95mm2, profi K08","1ks",146.96549650956945,{"$f":"F5575*(1-Elteq!$F$9)","v":146.96549650956945},"8591735023430"]
["TECHNIK","MHP 16/95 D",null,"Lisovací kleště s otočnými čelistmi na oka Cu DIN 16-95mm2 a AL 10-70mm2, profi K08D","1ks",146.96549650956945,{"$f":"F5576*(1-Elteq!$F$9)","v":146.96549650956945},"8591735023447"]
["TECHNIK","MHP 25/150",null,"Lisovací kleště s otočnými čelistmi na standardní Cu oka lehčená 25-150mm2, profi K09","1ks",179.995620725104,{"$f":"F5577*(1-Elteq!$F$9)","v":179.995620725104},"8591735023454"]
["TECHNIK","MHP 25/150 D",null,"Lisovací kleště s otočnými čelistmi na oka Cu DIN 25-150mm2 a AL 16-120mm2, profi K09D","1ks",183.70687063696181,{"$f":"F5578*(1-Elteq!$F$9)","v":183.70687063696181},"8591735023461"]
["TECHNIK","MHPL  6/50",null,"Lisovací kleště s otočnými čelistmi na standardní Cu oka lehčená 6-50mm2, economy","1ks",100.203747620161,{"$f":"F5579*(1-Elteq!$F$9)","v":100.203747620161},"8591735033224"]
["TECHNIK","MHPL  6/50 D",null,"Lisovací kleště s otočnými čelistmi na oka Cu DIN 6-50mm2 a AL 10-35mm2, economy","1ks",100.203747620161,{"$f":"F5580*(1-Elteq!$F$9)","v":100.203747620161},""]
["TECHNIK","MHPL 10/120",null,"Lisovací kleště s otočnými čelistmi na standardní Cu oka lehčená 10-120mm2, economy","1ks",118.75999717945007,{"$f":"F5581*(1-Elteq!$F$9)","v":118.75999717945007},""]
["TECHNIK","MHPL 10/120 D",null,"Lisovací kleště s otočnými čelistmi na oka Cu DIN 10-120mm2 a AL 10-95mm2, economy","1ks",118.75999717945007,{"$f":"F5582*(1-Elteq!$F$9)","v":118.75999717945007},""]
["TECHNIK","MHPL 25/150",null,"Lisovací kleště s otočnými čelistmi na standardní Cu oka lehčená 25-150mm2, economy","1ks",118.75999717945007,{"$f":"F5583*(1-Elteq!$F$9)","v":118.75999717945007},""]
["TECHNIK","MHPL 25/150 D",null,"Lisovací kleště s otočnými čelistmi na oka Cu DIN 25-150mm2 a AL 16-120mm2, economy","1ks",118.75999717945007,{"$f":"F5584*(1-Elteq!$F$9)","v":118.75999717945007},""]
["TECHNIK","MHPL 70/240 D",null,"Lisovací kleště s otočnými čelistmi na oka Cu DIN 70-240mm2 a AL 50-185mm2","1ks",272.73975602243081,{"$f":"F5585*(1-Elteq!$F$9)","v":272.73975602243081},"8591735055615"]
["TECHNIK","TN  70 SE",null,"Lisovací kleště na oka lehčená 6-70mm2, lisování trnem","1ks",213.39686993182434,{"$f":"F5586*(1-Elteq!$F$9)","v":213.39686993182434},"8591735008239"]
["TECHNIK","TN 120 SE",null,"Lisovací kleště na oka lehčená 6-120mm2, lisování trnem","1ks",259.41636883886122,{"$f":"F5587*(1-Elteq!$F$9)","v":259.41636883886122},"8591735008222"]
["TECHNIK","TNN  70",null,"Lisovací kleště na oka nylon 6-70mm2, lisování trnem","1ks",225.27286964976935,{"$f":"F5588*(1-Elteq!$F$9)","v":225.27286964976935},"8591735008253"]
["TECHNIK","TNN 120",null,"Lisovací kleště na oka nylon 6-120mm2, lisování trnem","1ks",276.48811843340718,{"$f":"F5589*(1-Elteq!$F$9)","v":276.48811843340718},"8591735008246"]
["TECHNIK","LK1",null,"9743200A KNIPEX lisovací kleště na kabelové koncovky bez čelistí, Tyco 539635-1 Ergocrimp","1ks",92.038997814073795,{"$f":"F5590*(1-Elteq!$F$9)","v":92.038997814073795},"8591735018535"]
["TECHNIK","LK1 CHROM",null,"9743200A KNIPEX lisovací kleště na kabelové koncovky bez čelistí, Tyco 539635-1 chromované","1ks",97.234747690674737,{"$f":"F5591*(1-Elteq!$F$9)","v":97.234747690674737},"8591735049409"]
["TECHNIK","LK-2",null,"Lisovací kleště na kabelové koncovky bez čelistí, economy (pro čelisti C2)","1ks",15.958374620988602,{"$f":"F5592*(1-Elteq!$F$9)","v":15.958374620988602},"8591735008260"]
["TECHNIK","LK-2KY",null,"Lisovací kleště na kabelové koncovky bez čelistí, delší rukojeti (pro čelisti C2Y)","1ks",44.906123933479556,{"$f":"F5593*(1-Elteq!$F$9)","v":44.906123933479556},"8591735023911"]
["TECHNIK","LK-2P",null,"Lisovací kleště na kabelové koncovky bez čelistí, profi (pro čelisti C2)","1ks",33.030124215534549,{"$f":"F5594*(1-Elteq!$F$9)","v":33.030124215534549},"8591735010751"]
["TECHNIK","LK-2TF",null,"Lisovací kleště na kabelové koncovky bez čelistí, robustní (pro čelisti C2)","1ks",53.627561226345421,{"$f":"F5595*(1-Elteq!$F$9)","v":53.627561226345421},"8591735018894"]
["TECHNIK","LK-2TF PLUS",null,"Lisovací kleště na kabelové koncovky bez čelistí, robustní s páčkami (pro čelisti C2)","1ks",60.864498554468156,{"$f":"F5596*(1-Elteq!$F$9)","v":60.864498554468156},"8591735018900"]
["TECHNIK","LK-2Z",null,"Lisovací kleště na kabelové koncovky bez čelistí, zahnuté, economy (pro čelisti C2)","1ks",20.411874515217981,{"$f":"F5597*(1-Elteq!$F$9)","v":20.411874515217981},"8591735048891"]
["TECHNIK","LK-3",null,"Lisovací kleště na kabelové koncovky - bez lisovacích čelistí","1ks",210.4278700023381,{"$f":"F5598*(1-Elteq!$F$9)","v":210.4278700023381},"8591735023928"]
["TECHNIK","LK-CC",null,"Lisovací kleště CLICK\"N\"CRIMP se třemi páry zasouvacích čelistí (K507)","1sada",134.53280930484578,{"$f":"F5599*(1-Elteq!$F$9)","v":134.53280930484578},"8591735032906"]
["TECHNIK","LK-CC/0",null,"Lisovací kleště CLICK\"N\"CRIMP - bez lisovacích čelistí","1ks",87.585497919844428,{"$f":"F5600*(1-Elteq!$F$9)","v":87.585497919844428},"8591735034986"]
["TECHNIK","LKT1",null,"Stolní držák pro lisovací kleště na kabelové koncovky LK1 - bez kleští !","1ks",59.008873598539253,{"$f":"F5601*(1-Elteq!$F$9)","v":59.008873598539253},"8591735049416"]
["TECHNIK","LR SET 5",null,"973302 KNIPEX lisovací kleště LR s 5-ti zasouvacími čelistmi, kvalitní provedení MultiCrimp","1sada",245.87030666058021,{"$f":"F5602*(1-Elteq!$F$9)","v":245.87030666058021},""]
["TECHNIK","KN 97 90 00",null,"979000 KNIPEX sada kabelových koncovek s lisovacími kleštěmi","1sada",202.89403268126674,{"$f":"F5603*(1-Elteq!$F$9)","v":202.89403268126674},""]
["TECHNIK","KN 97 90 00 LE",null,"979000LE KNIPEX kufr prázdný pro uložení kabelových koncovek a lisovacích kleští","1ks",49.062723834760305,{"$f":"F5604*(1-Elteq!$F$9)","v":49.062723834760305},""]
["TECHNIK","KN 97 90 01",null,"979001 KNIPEX sada kabelových koncovek s lisovacími kleštěmi","1sada",147.26239650251807,{"$f":"F5605*(1-Elteq!$F$9)","v":147.26239650251807},""]
["TECHNIK","KN 97 90 05",null,"979005 KNIPEX sada neizolovaných dutinek 0,5-16mm2 s lisovacími kleštěmi","1sada",115.04874726759225,{"$f":"F5606*(1-Elteq!$F$9)","v":115.04874726759225},""]
["TECHNIK","KN 97 90 06",null,"979006 KNIPEX sada izolovaných dutinek 0,5-16mm2 s lisovacími kleštěmi","1sada",129.11438443353336,{"$f":"F5607*(1-Elteq!$F$9)","v":129.11438443353336},""]
["TECHNIK","KN 97 90 09",null,"979009 KNIPEX sada izolovaných dutinek 0,5-10mm2 s lisovacími kleštěmi","1sada",262.64515626217752,{"$f":"F5608*(1-Elteq!$F$9)","v":262.64515626217752},""]
["TECHNIK","KN 97 90 10",null,"979010 KNIPEX sada izolovaných dutinek 0,5-10mm2 s odizolovacími a lisovacími kleštěmi","1sada",344.99779180630242,{"$f":"F5609*(1-Elteq!$F$9)","v":344.99779180630242},""]
["TECHNIK","KN 97 90 12",null,"979012 KNIPEX sada izolovaných dutinek 0,5-10mm2 s odizolovacími a lisovacími kleštěmi","1sada",343.32772934596642,{"$f":"F5610*(1-Elteq!$F$9)","v":343.32772934596642},""]
["TECHNIK","KN 97 90 21",null,"979021 KNIPEX sada kabelových koncovek s lisovacími kleštěmi","1sada",220.81936975553998,{"$f":"F5611*(1-Elteq!$F$9)","v":220.81936975553998},""]
["TECHNIK","KN 97 90 22",null,"979022 KNIPEX sada kabelových koncovek s odizolovacími a lisovacími kleštěmi","1sada",322.95296732986702,{"$f":"F5612*(1-Elteq!$F$9)","v":322.95296732986702},""]
["TECHNIK","KN 97 90 23",null,"979023 KNIPEX sada izolovaných dutinek 0,5-6mm2 s lisovacími kleštěmi","1sada",205.08367012926283,{"$f":"F5613*(1-Elteq!$F$9)","v":205.08367012926283},""]
["TECHNIK","KN 97 90 24",null,"979024 KNIPEX sada izolovaných dutinek 0,5-10mm2 s odizolovacími a lisovacími kleštěmi","1sada",364.14784135148875,{"$f":"F5614*(1-Elteq!$F$9)","v":364.14784135148875},""]
["TECHNIK","KN 97 90 25",null,"979025 KNIPEX sada kabelových koncovek s lisovacími kleštěmi","1sada",118.31464719002713,{"$f":"F5615*(1-Elteq!$F$9)","v":118.31464719002713},""]
["TECHNIK","KY-SET",null,"Kufřík s lisovacími kleštěmi KY a sadou 7 lisovacích čelistí","1sada",101.31712259371834,{"$f":"F5616*(1-Elteq!$F$9)","v":101.31712259371834},"8591735052874"]
["TECHNIK","LB-SET 10",null,"Kufřík s lisovacími kleštěmi LB a sadou 10-ti lisovacích čelistí, dostupné 9/2013","1sada",164.40837109530119,{"$f":"F5617*(1-Elteq!$F$9)","v":164.40837109530119},""]
["TECHNIK","LB-SET 5",null,"Kufřík s lisovacími kleštěmi LB a sadou 5-ti lisovacích čelistí, dostupné 9/2013","1sada",94.265747761188493,{"$f":"F5618*(1-Elteq!$F$9)","v":94.265747761188493},""]
["TECHNIK","LF-SET",null,"Kufřík s lisovacími zahnutými kleštěmi LKZ a sadou 5-ti lisovacích čelistí typu C2","1sada",55.29762368668144,{"$f":"F5619*(1-Elteq!$F$9)","v":55.29762368668144},"8591735050115"]
["TECHNIK","LH-SET",null,"Kufřík s lisovacími kleštěmi LK2 a sadou 5-ti lisovacích čelistí","1sada",55.29762368668144,{"$f":"F5620*(1-Elteq!$F$9)","v":55.29762368668144},"8591735033460"]
["TECHNIK","LZ-SET",null,"Kufřík s lisovacími zahnutými kleštěmi LZ a sadou 5-ti lisovacích čelistí","1sada",53.07087373956675,{"$f":"F5621*(1-Elteq!$F$9)","v":53.07087373956675},""]
["TECHNIK","SK 05",null,"Kovový kufr ke kleštím K 05, MHP 6/50","1ks",107.62624744387662,{"$f":"F5622*(1-Elteq!$F$9)","v":107.62624744387662},"8591735032715"]
["TECHNIK","SK 06",null,"Kovový kufr ke kleštím K 06/09, MHP 10/120, 25/150","1ks",167.00624603360166,{"$f":"F5623*(1-Elteq!$F$9)","v":167.00624603360166},"8591735032722"]
["TECHNIK","SK-COMBI NET",null,"Kufřík s lisovacími kleštěmi a sadou modulárních konektorů","1sada",107.25512245269084,{"$f":"F5624*(1-Elteq!$F$9)","v":107.25512245269084},"8591735014285"]
["TECHNIK","SK-KM",null,"Malý sevisní kufřík kovový prázdný (MKM)","1ks",32.102311737570098,{"$f":"F5625*(1-Elteq!$F$9)","v":32.102311737570098},"8591735032708"]
["TECHNIK","SK-KM-DI 054",null,"Kufřík vč. kleští s dutinkami izolovanými 0,5-4mm2 (MKQ-DI)","1sada",337.72374197906112,{"$f":"F5626*(1-Elteq!$F$9)","v":337.72374197906112},""]
["TECHNIK","SK-KM-DN 054",null,"Kufřík vč. kleští s dutinkami neizol. 0,5-4mm2 (MKQ-DN)","1sada",324.73436728755877,{"$f":"F5627*(1-Elteq!$F$9)","v":324.73436728755877},""]
["TECHNIK","SK-KV",null,"Velký sevisní kufřík kovový prázdný (MKV)","1ks",40.823749030435962,{"$f":"F5628*(1-Elteq!$F$9)","v":40.823749030435962},"8591735032692"]
["TECHNIK","SK-LK1",null,"9743200 KNIPEX kufřík s profi lisovacími kleštěmi LK-1 bez čelistí, (LUS 1)","1sada",148.26443397871969,{"$f":"F5629*(1-Elteq!$F$9)","v":148.26443397871969},"8591735032685"]
["TECHNIK","SK-MOST 2",null,"Servisní kufřík MOST","1sada",824.08304292802768,{"$f":"F5630*(1-Elteq!$F$9)","v":824.08304292802768},"8591735032678"]
["TECHNIK","SK-PM",null,"Malý sevisní kufřík plastový prázdný","1ks",38.968124074507053,{"$f":"F5631*(1-Elteq!$F$9)","v":38.968124074507053},"8591735027803"]
["TECHNIK","SK-PM-MO 056",null,"Kufřík vč. kleští s konektory mosaznými 0,5-6mm2","1sada",103.54387254083302,{"$f":"F5632*(1-Elteq!$F$9)","v":103.54387254083302},""]
["TECHNIK","SK-PM-MOC 056",null,"Kufřík s kleštěmi a konektory cínovanými 0,5-6mm2","1sada",109.48187239980552,{"$f":"F5633*(1-Elteq!$F$9)","v":109.48187239980552},""]
["TECHNIK","SK-PROFI CRIMP",null,"Sada 5-ti čelistí s PROFI lisovacími kleštěmi","1sada",123.39905956927234,{"$f":"F5634*(1-Elteq!$F$9)","v":123.39905956927234},"8591735014292"]
["TECHNIK","SK-PROFI CRIMP NET",null,"Kufřík s profi lisovacími kleštěmi a sadou 8-mi lisovacích čelistí","1sada",138.42962171229649,{"$f":"F5635*(1-Elteq!$F$9)","v":138.42962171229649},""]
["TECHNIK","SK-PV",null,"Velký sevisní kufřík plastový prázdný","1ks",40.823749030435962,{"$f":"F5636*(1-Elteq!$F$9)","v":40.823749030435962},"8591735032739"]
["TECHNIK","SK-PV-OI 056",null,"Kufřík s kleštěmi a kabelovými oky izolovanými 0,5-6mm2","1sada",117.64662220589273,{"$f":"F5637*(1-Elteq!$F$9)","v":117.64662220589273},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"SK-PV-ON 056",null,"Kufřík s kleštěmi a kabelovými oky neizolovanými 0,5-6mm2","1sada",134.53280930484578,{"$f":"F5638*(1-Elteq!$F$9)","v":134.53280930484578},""]
["TECHNIK","SK-SOLAR H&S",null,"Servisní kufřík s nástroji pro solární konektory HUBER & SUHNER","1sada",459.82386407918324,{"$f":"F5639*(1-Elteq!$F$9)","v":459.82386407918324},"8591735032661"]
["TECHNIK","SK-SOLAR MC",null,"Servisní kufřík s nástroji pro solární konektory MC3 a MC4","1sada",632.76810997175744,{"$f":"F5640*(1-Elteq!$F$9)","v":632.76810997175744},"8591735032654"]
["TECHNIK","SK-SOLAR TYCO",null,"Servisní kufřík s nástroji pro solární konektory TYCO","1sada",486.91598843574525,{"$f":"F5641*(1-Elteq!$F$9)","v":486.91598843574525},"8591735032647"]
["TECHNIK","SK-SOLAR UNI",null,"Servisní kufřík s nástroji pro nejpoužívanější typy solárních konektorů","1sada",743.36335734512022,{"$f":"F5642*(1-Elteq!$F$9)","v":743.36335734512022},"8591735032630"]
["TECHNIK","SK-TF",null,"Kufřík s profi lisovacími kleštěmi LK-2TF bez čelistí","1sada",78.307373140199886,{"$f":"F5643*(1-Elteq!$F$9)","v":78.307373140199886},"8591735018917"]
["TECHNIK","SK-TF 5",null,"Kufřík s profi lisovacími kleštěmi LK-2TF a sadou 5-ti lisovacích čelistí (LU SET)","1sada",171.45974592783102,{"$f":"F5644*(1-Elteq!$F$9)","v":171.45974592783102},"8591735018948"]
["TECHNIK","SK-TF PLUS",null,"Kufřík s profi lisovacími kleštěmi LK-2TF PLUS bez čelistí","1sada",84.98762298154395,{"$f":"F5645*(1-Elteq!$F$9)","v":84.98762298154395},"8591735018924"]
["TECHNIK","SK-TF PLUS 5",null,"Kufřík s profi lisovacími kleštěmi LK-2TF PLUS a sadou 5-ti lisovacích čelistí (LU SET)","1sada",181.10899569866135,{"$f":"F5646*(1-Elteq!$F$9)","v":181.10899569866135},"8591735018931"]
["TECHNIK","Tool Box",null,"10503817 profesionální box IRWIN na nářadí z odolného plastu 26\" rozměry 700x300x300mm","1ks",80.162998096128788,{"$f":"F5647*(1-Elteq!$F$9)","v":80.162998096128788},""]
["TECHNIK","KN 98 00 08",null,"980008 KNIPEX jednostranný otevřený klíč izolovaný do 1000V, velikost 8","1ks",15.216124638617039,{"$f":"F5648*(1-Elteq!$F$9)","v":15.216124638617039},""]
["TECHNIK","KN 98 00 10",null,"980010 KNIPEX jednostranný otevřený klíč izolovaný do 1000V, velikost 10","1ks",16.329499612174384,{"$f":"F5649*(1-Elteq!$F$9)","v":16.329499612174384},""]
["TECHNIK","KN 98 00 12",null,"980012 KNIPEX jednostranný otevřený klíč izolovaný do 1000V, velikost 12","1ks",16.960412097190211,{"$f":"F5650*(1-Elteq!$F$9)","v":16.960412097190211},""]
["TECHNIK","KN 98 00 17",null,"980017 KNIPEX jednostranný otevřený klíč izolovaný do 1000V, velikost 17","1ks",19.892299527557885,{"$f":"F5651*(1-Elteq!$F$9)","v":19.892299527557885},""]
["TECHNIK","KN 98 00 18",null,"980018 KNIPEX jednostranný otevřený klíč izolovaný do 1000V, velikost 18","1ks",22.081936975553997,{"$f":"F5652*(1-Elteq!$F$9)","v":22.081936975553997},""]
["TECHNIK","KN 98 00 19",null,"980019 KNIPEX jednostranný otevřený klíč izolovaný do 1000V, velikost 19","1ks",22.081936975553997,{"$f":"F5653*(1-Elteq!$F$9)","v":22.081936975553997},""]
["TECHNIK","KN 98 00 22",null,"980022 KNIPEX jednostranný otevřený klíč izolovaný do 1000V, velikost 22","1ks",23.714886936771435,{"$f":"F5654*(1-Elteq!$F$9)","v":23.714886936771435},""]
["TECHNIK","KN 98 00 24",null,"980024 KNIPEX jednostranný otevřený klíč izolovaný do 1000V, velikost 24","1ks",26.275649375953329,{"$f":"F5655*(1-Elteq!$F$9)","v":26.275649375953329},""]
["TECHNIK","KN 98 00 27",null,"980027 KNIPEX jednostranný otevřený klíč izolovaný do 1000V, velikost 27","1ks",28.539511822186594,{"$f":"F5656*(1-Elteq!$F$9)","v":28.539511822186594},"8591735045616"]
["TECHNIK","KN 98 01 13",null,"980113 KNIPEX jednostranný očkový klíč izolovaný do 1000V, velikost 13","1ks",21.265461994945277,{"$f":"F5657*(1-Elteq!$F$9)","v":21.265461994945277},""]
["TECHNIK","KN 98 01 17",null,"980117 KNIPEX jednostranný očkový klíč izolovaný do 1000V, velikost 17","1ks",25.347836897988874,{"$f":"F5658*(1-Elteq!$F$9)","v":25.347836897988874},""]
["TECHNIK","KN 98 03 055",null,"9803055 KNIPEX nástrčkový klíč s rukojetí izolovaný do 1000V, vnitřní šestihran velikost 5,5mm","1ks",13.063599689739508,{"$f":"F5659*(1-Elteq!$F$9)","v":13.063599689739508},""]
["TECHNIK","KN 98 03 07",null,"980307 KNIPEX nástrčkový klíč s rukojetí izolovaný do 1000V, vnitřní šestihran velikost 7mm","1ks",14.770774649194102,{"$f":"F5660*(1-Elteq!$F$9)","v":14.770774649194102},""]
["TECHNIK","KN 98 03 08",null,"980308 KNIPEX nástrčkový klíč s rukojetí izolovaný do 1000V, vnitřní šestihran velikost 8mm","1ks",14.770774649194102,{"$f":"F5661*(1-Elteq!$F$9)","v":14.770774649194102},""]
["TECHNIK","KN 98 03 10",null,"980310 KNIPEX nástrčkový klíč s rukojetí izolovaný do 1000V, vnitřní šestihran velikost 10mm","1ks",15.327462135972775,{"$f":"F5662*(1-Elteq!$F$9)","v":15.327462135972775},""]
["TECHNIK","KN 98 14 05",null,"981405 KNIPEX klíč Imbus s pevnou T-rukojetí izolovaný do 1000V, délka 120mm, velikost 5","1ks",36.333136637088003,{"$f":"F5663*(1-Elteq!$F$9)","v":36.333136637088003},""]
["TECHNIK","KN 98 14 06",null,"981406 KNIPEX klíč Imbus s pevnou T-rukojetí izolovaný do 1000V, délka 120mm, velikost 6","1ks",36.333136637088003,{"$f":"F5664*(1-Elteq!$F$9)","v":36.333136637088003},""]
["TECHNIK","KN 98 14 08",null,"981408 KNIPEX klíč Imbus s pevnou T-rukojetí izolovaný do 1000V, délka 120mm, velikost 8","1ks",36.333136637088003,{"$f":"F5665*(1-Elteq!$F$9)","v":36.333136637088003},""]
["TECHNIK","KN 98 39 06",null,"983906 KNIPEX nástrčkový klíč 3/8\" izolovaný do 1000V, vnitřní šestihran, velikost 6mm","1ks",32.770336721704503,{"$f":"F5666*(1-Elteq!$F$9)","v":32.770336721704503},"8591735045609"]
["TECHNIK","KN 98 40",null,"9840 KNIPEX příčná rukojeť 1/2\" izolovaná do 1000V typ \"T\"","1ks",49.508073824183249,{"$f":"F5667*(1-Elteq!$F$9)","v":49.508073824183249},""]
["TECHNIK","KN 98 41",null,"9841 KNIPEX ráčna 1/2\" izolovaná do 1000V přepínatelná","1ks",100.46353511399104,{"$f":"F5668*(1-Elteq!$F$9)","v":100.46353511399104},""]
["TECHNIK","KN 98 42",null,"9842 KNIPEX ráčna 1/2\" izolovaná do 1000V přestavitelná","1ks",101.79958508225985,{"$f":"F5669*(1-Elteq!$F$9)","v":101.79958508225985},""]
["TECHNIK","KN 98 43 50",null,"984350 KNIPEX momentový klíč 1/2\" izolovaný do 1000V délka 385mm, rozsah 5-50Nm","1ks",324.36324229637302,{"$f":"F5670*(1-Elteq!$F$9)","v":324.36324229637302},""]
["TECHNIK","KN 98 45 125",null,"9845125 KNIPEX prodlužovací nástavec 1/2\" izolovaný do 1000V, délka 125mm","1ks",36.59292413091805,{"$f":"F5671*(1-Elteq!$F$9)","v":36.59292413091805},""]
["TECHNIK","KN 98 45 250",null,"9845250 KNIPEX prodlužovací nástavec 1/2\" izolovaný do 1000V, délka 250mm","1ks",39.673261557760036,{"$f":"F5672*(1-Elteq!$F$9)","v":39.673261557760036},""]
["TECHNIK","KN 98 47 10",null,"984710 KNIPEX nástrčný klíč 1/2\" izolovaný do 1000V, velikost 10","1ks",15.958374620988602,{"$f":"F5673*(1-Elteq!$F$9)","v":15.958374620988602},""]
["TECHNIK","KN 98 47 11",null,"984711 KNIPEX nástrčný klíč 1/2\" izolovaný do 1000V, velikost 11","1ks",15.958374620988602,{"$f":"F5674*(1-Elteq!$F$9)","v":15.958374620988602},""]
["TECHNIK","KN 98 47 12",null,"984712 KNIPEX nástrčný klíč 1/2\" izolovaný do 1000V, velikost 12","1ks",15.958374620988602,{"$f":"F5675*(1-Elteq!$F$9)","v":15.958374620988602},""]
["TECHNIK","KN 98 47 13",null,"984713 KNIPEX nástrčný klíč 1/2\" izolovaný do 1000V, velikost 13","1ks",15.958374620988602,{"$f":"F5676*(1-Elteq!$F$9)","v":15.958374620988602},""]
["TECHNIK","KN 98 47 14",null,"984714 KNIPEX nástrčný klíč 1/2\" izolovaný do 1000V, velikost 14","1ks",15.958374620988602,{"$f":"F5677*(1-Elteq!$F$9)","v":15.958374620988602},""]
["TECHNIK","KN 98 47 16",null,"984716 KNIPEX nástrčný klíč 1/2\" izolovaný do 1000V, velikost 16","1ks",16.886187098953055,{"$f":"F5678*(1-Elteq!$F$9)","v":16.886187098953055},""]
["TECHNIK","KN 98 47 17",null,"984717 KNIPEX nástrčný klíč 1/2\" izolovaný do 1000V, velikost 17","1ks",16.886187098953055,{"$f":"F5679*(1-Elteq!$F$9)","v":16.886187098953055},""]
["TECHNIK","KN 98 47 18",null,"984718 KNIPEX nástrčný klíč 1/2\" izolovaný do 1000V, velikost 18","1ks",17.554212083087464,{"$f":"F5680*(1-Elteq!$F$9)","v":17.554212083087464},""]
["TECHNIK","KN 98 47 19",null,"984719 KNIPEX nástrčný klíč 1/2\" izolovaný do 1000V, velikost 19","1ks",17.9995620725104,{"$f":"F5681*(1-Elteq!$F$9)","v":17.9995620725104},""]
["TECHNIK","KN 98 47 22",null,"984722 KNIPEX nástrčný klíč 1/2\" izolovaný do 1000V, velikost 22","1ks",21.042787000233808,{"$f":"F5682*(1-Elteq!$F$9)","v":21.042787000233808},""]
["TECHNIK","KN 98 47 24",null,"984724 KNIPEX nástrčný klíč 1/2\" izolovaný do 1000V, velikost 24","1ks",21.376799492301011,{"$f":"F5683*(1-Elteq!$F$9)","v":21.376799492301011},""]
["TECHNIK","KN 98 47 27",null,"984727 KNIPEX nástrčný klíč 1/2\" izolovaný do 1000V, velikost 27","1ks",22.527286964976934,{"$f":"F5684*(1-Elteq!$F$9)","v":22.527286964976934},""]
["TECHNIK","KN 98 49 05",null,"984905 KNIPEX nástrčkový klíč 1/2\" izolovaný do 1000V, vnitřní šestihran velikost 5mm","1ks",28.836411815135218,{"$f":"F5685*(1-Elteq!$F$9)","v":28.836411815135218},"8591735045623"]
["TECHNIK","KN 98 49 06",null,"984906 KNIPEX nástrčkový klíč 1/2\" izolovaný do 1000V, vnitřní šestihran velikost 6mm","1ks",28.836411815135218,{"$f":"F5686*(1-Elteq!$F$9)","v":28.836411815135218},"8591735045630"]
["TECHNIK","KN 98 49 08",null,"984908 KNIPEX nástrčkový klíč 1/2\" izolovaný do 1000V, vnitřní šestihran velikost 8mm","1ks",28.836411815135218,{"$f":"F5687*(1-Elteq!$F$9)","v":28.836411815135218},"8591735045647"]
["TECHNIK","KN 98 65 40",null,"986540 KNIPEX elektrikářské rukavice izolované do 1000V, velikost 9","1ks",55.668748677867221,{"$f":"F5688*(1-Elteq!$F$9)","v":55.668748677867221},""]
["TECHNIK","KN 98 65 41",null,"986541 KNIPEX elektrikářské rukavice izolované do 1000V, velikost 10","1ks",58.452186111760582,{"$f":"F5689*(1-Elteq!$F$9)","v":58.452186111760582},""]
["TECHNIK","KN 98 99 11",null,"989911 KNIPEX sada izolovaného nářadí do 1000V, 17 dílů","1ks",490.66435084672167,{"$f":"F5690*(1-Elteq!$F$9)","v":490.66435084672167},""]
["TECHNIK","KN 98 99 12",null,"989912 KNIPEX sada izolovaného nářadí do 1000V, 26 dílů","1ks",599.70087325710426,{"$f":"F5691*(1-Elteq!$F$9)","v":599.70087325710426},""]
["TECHNIK","KN 98 99 13",null,"989913 KNIPEX sada izolovaného nářadí do 1000V, 15 dílů","1ks",344.99779180630242,{"$f":"F5692*(1-Elteq!$F$9)","v":344.99779180630242},""]
["TECHNIK","ST kombi 1",null,"Bit pro kombinované šrouby, velikost 1, délka 50mm","1ks",3.7483624109763927,{"$f":"F5693*(1-Elteq!$F$9)","v":3.7483624109763927},""]
["TECHNIK","ST kombi 2",null,"Bit pro kombinované šrouby, velikost 2, délka 50mm","1ks",3.7483624109763927,{"$f":"F5694*(1-Elteq!$F$9)","v":3.7483624109763927},""]
["TECHNIK","WR 003544",null,"Sada ráčny 8100 SA Zyklop 1/4 Starter-Set WERA","1ks",99.721285131619481,{"$f":"F5695*(1-Elteq!$F$9)","v":99.721285131619481},""]
["TECHNIK","WR 052490",null,"Držák bitů WERA s rychloupínací hlavou a magnetem","1ks",20.560324511692293,{"$f":"F5696*(1-Elteq!$F$9)","v":20.560324511692293},""]
["TECHNIK","WR 052502",null,"Držák bitů WERA s rychloupínací hlavou a magnetem","1ks",15.958374620988602,{"$f":"F5697*(1-Elteq!$F$9)","v":15.958374620988602},""]
["TECHNIK","WR 053457",null,"Držák bitů WERA se zajišťovacím kroužkem a magnetem","1ks",4.6390623898222678,{"$f":"F5698*(1-Elteq!$F$9)","v":4.6390623898222678},""]
["TECHNIK","WR 053459",null,"Držák bitů WERA se zajišťovacím kroužkem a magnetem","1ks",17.220199591020261,{"$f":"F5699*(1-Elteq!$F$9)","v":17.220199591020261},""]
["TECHNIK","WR 056168",null,"Sada bitů WERA Hex-Plus s rychloupínacím držákem - 7 dílů","1sada",24.123124427075794,{"$f":"F5700*(1-Elteq!$F$9)","v":24.123124427075794},""]
["TECHNIK","WR 056200",null,"Bit WERA pro šrouby s drážkou 0,5x3,0mm - houževnatý","1ks",0.85358747972729732,{"$f":"F5701*(1-Elteq!$F$9)","v":0.85358747972729732},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"WR 056295",null,"Sada bitů WERA s rychloupínacím držákem - 7 dílů","1sada",8.2389748043243483,{"$f":"F5702*(1-Elteq!$F$9)","v":8.2389748043243483},""]
["TECHNIK","WR 056303",null,"Bit WERA pro šrouby s profilem Hex-Plus 1,5mm","1ks",1.8927374550474854,{"$f":"F5703*(1-Elteq!$F$9)","v":1.8927374550474854},""]
["TECHNIK","WR 056305",null,"Bit WERA pro šrouby s profilem Hex-Plus 2,0mm","1ks",1.8927374550474854,{"$f":"F5704*(1-Elteq!$F$9)","v":1.8927374550474854},""]
["TECHNIK","WR 056310",null,"Bit WERA pro šrouby s profilem Hex-Plus 2,5mm","1ks",1.8927374550474854,{"$f":"F5705*(1-Elteq!$F$9)","v":1.8927374550474854},""]
["TECHNIK","WR 056315",null,"Bit WERA pro šrouby s profilem Hex-Plus 3,0mm","1ks",1.8927374550474854,{"$f":"F5706*(1-Elteq!$F$9)","v":1.8927374550474854},""]
["TECHNIK","WR 056320",null,"Bit WERA pro šrouby s profilem Hex-Plus 4,0mm","1ks",1.8927374550474854,{"$f":"F5707*(1-Elteq!$F$9)","v":1.8927374550474854},""]
["TECHNIK","WR 056325",null,"Bit WERA pro šrouby s profilem Hex-Plus 5,0mm","1ks",1.8927374550474854,{"$f":"F5708*(1-Elteq!$F$9)","v":1.8927374550474854},""]
["TECHNIK","WR 056330",null,"Bit WERA pro šrouby s profilem Hex-Plus 6,0mm","1ks",1.8927374550474854,{"$f":"F5709*(1-Elteq!$F$9)","v":1.8927374550474854},""]
["TECHNIK","WR 056332",null,"Bit WERA pro šrouby s profilem Hex-Plus 7,0mm","1ks",2.7092124356562048,{"$f":"F5710*(1-Elteq!$F$9)","v":2.7092124356562048},""]
["TECHNIK","WR 056335",null,"Bit WERA pro šrouby s profilem Hex-Plus 8,0mm","1ks",2.7092124356562048,{"$f":"F5711*(1-Elteq!$F$9)","v":2.7092124356562048},""]
["TECHNIK","WR 056340",null,"Bit WERA pro šrouby s profilem Hex-Plus 10,0mm","1ks",2.7092124356562048,{"$f":"F5712*(1-Elteq!$F$9)","v":2.7092124356562048},""]
["TECHNIK","WR 056500",null,"Bit WERA pro křížové šrouby PH 0 - houževnatý","1ks",1.0762624744387663,{"$f":"F5713*(1-Elteq!$F$9)","v":1.0762624744387663},""]
["TECHNIK","WR 056505",null,"Bit WERA pro křížové šrouby PH 1 - houževnatý","1ks",1.0762624744387663,{"$f":"F5714*(1-Elteq!$F$9)","v":1.0762624744387663},""]
["TECHNIK","WR 056507",null,"Bit WERA pro křížové šrouby PH 1","1ks",1.7628437081324619,{"$f":"F5715*(1-Elteq!$F$9)","v":1.7628437081324619},""]
["TECHNIK","WR 056510",null,"Bit WERA pro křížové šrouby PH 2 - houževnatý","1ks",1.0762624744387663,{"$f":"F5716*(1-Elteq!$F$9)","v":1.0762624744387663},""]
["TECHNIK","WR 056525",null,"Bit WERA pro křížové šrouby PH 3 - houževnatý","1ks",1.0762624744387663,{"$f":"F5717*(1-Elteq!$F$9)","v":1.0762624744387663},""]
["TECHNIK","WR 056605",null,"Bit WERA pro křížové šrouby PH 1 - extra tvrdý","1ks",1.0762624744387663,{"$f":"F5718*(1-Elteq!$F$9)","v":1.0762624744387663},"8591735022648"]
["TECHNIK","WR 056610",null,"Bit WERA pro křížové šrouby PH 2 - extra tvrdý","1ks",1.0762624744387663,{"$f":"F5719*(1-Elteq!$F$9)","v":1.0762624744387663},"8591735022655"]
["TECHNIK","WR 056625",null,"Bit WERA pro křížové šrouby PH 3 - extra tvrdý","1ks",1.0762624744387663,{"$f":"F5720*(1-Elteq!$F$9)","v":1.0762624744387663},""]
["TECHNIK","WR 056910",null,"Bit WERA pro křížové šrouby PZ 1 - extra tvrdý","1ks",1.0762624744387663,{"$f":"F5721*(1-Elteq!$F$9)","v":1.0762624744387663},"8591735033156"]
["TECHNIK","WR 056915",null,"Bit WERA pro křížové šrouby PZ 2 - extra tvrdý","1ks",1.0762624744387663,{"$f":"F5722*(1-Elteq!$F$9)","v":1.0762624744387663},"8591735033163"]
["TECHNIK","WR 056925",null,"Bit WERA pro křížové šrouby PZ 3 - extra tvrdý","1ks",1.0762624744387663,{"$f":"F5723*(1-Elteq!$F$9)","v":1.0762624744387663},"8591735036867"]
["TECHNIK","WR 057126",null,"Sada bitů WERA s rychloupínacím držákem - 31 dílů","1sada",24.828261910328781,{"$f":"F5724*(1-Elteq!$F$9)","v":24.828261910328781},""]
["TECHNIK","WR 057705",null,"Bit 5/16\" pro křížové šrouby PH 1","1ks",4.1194874021621741,{"$f":"F5725*(1-Elteq!$F$9)","v":4.1194874021621741},""]
["TECHNIK","WR 060110",null,"Bit WERA pro šrouby s profilem TORX - TX 20 x 70mm","1ks",4.045262403925018,{"$f":"F5726*(1-Elteq!$F$9)","v":4.045262403925018},""]
["TECHNIK","WR 060402",null,"Nástavec nástrčný WERA rozměr 7,0x50mm","1ks",3.2287874233162985,{"$f":"F5727*(1-Elteq!$F$9)","v":3.2287874233162985},""]
["TECHNIK","WR 060403",null,"Nástavec nástrčný WERA rozměr 8,0x50mm","1ks",3.2287874233162985,{"$f":"F5728*(1-Elteq!$F$9)","v":3.2287874233162985},""]
["TECHNIK","WR 066485",null,"Bit WERA pro šrouby s profilem TORX - TX 10 x 25mm","1ks",1.0762624744387663,{"$f":"F5729*(1-Elteq!$F$9)","v":1.0762624744387663},""]
["TECHNIK","WR 066486",null,"Bit WERA pro šrouby s profilem TORX - TX 15 x 25mm","1ks",1.0762624744387663,{"$f":"F5730*(1-Elteq!$F$9)","v":1.0762624744387663},""]
["TECHNIK","WR 066487",null,"Bit WERA pro šrouby s profilem TORX - TX 20 x 25mm","1ks",1.0762624744387663,{"$f":"F5731*(1-Elteq!$F$9)","v":1.0762624744387663},""]
["TECHNIK","WR 066488",null,"Bit WERA pro šrouby s profilem TORX - TX 25","1ks",1.0762624744387663,{"$f":"F5732*(1-Elteq!$F$9)","v":1.0762624744387663},""]
["TECHNIK","WR 066489",null,"Bit WERA pro šrouby s profilem TORX - TX 27","1ks",1.0762624744387663,{"$f":"F5733*(1-Elteq!$F$9)","v":1.0762624744387663},""]
["TECHNIK","WR 066490",null,"Bit WERA pro šrouby s profilem TORX - TX 30","1ks",1.0762624744387663,{"$f":"F5734*(1-Elteq!$F$9)","v":1.0762624744387663},""]
["TECHNIK","WR 066491",null,"Bit WERA pro šrouby s profilem TORX - TX 40","1ks",1.0762624744387663,{"$f":"F5735*(1-Elteq!$F$9)","v":1.0762624744387663},""]
["TECHNIK","WR 066492",null,"Bit WERA pro šrouby s profilem TORX - TX 5","1ks",1.2803812195909461,{"$f":"F5736*(1-Elteq!$F$9)","v":1.2803812195909461},""]
["TECHNIK","WR 066493",null,"Bit WERA pro šrouby s profilem TORX - TX 6","1ks",1.2803812195909461,{"$f":"F5737*(1-Elteq!$F$9)","v":1.2803812195909461},""]
["TECHNIK","WR 066494",null,"Bit WERA pro šrouby s profilem TORX - TX 7","1ks",1.2803812195909461,{"$f":"F5738*(1-Elteq!$F$9)","v":1.2803812195909461},""]
["TECHNIK","WR 066495",null,"Bit WERA pro šrouby s profilem TORX - TX 8","1ks",1.2803812195909461,{"$f":"F5739*(1-Elteq!$F$9)","v":1.2803812195909461},""]
["TECHNIK","WR 066496",null,"Bit WERA pro šrouby s profilem TORX - TX 9","1ks",1.2803812195909461,{"$f":"F5740*(1-Elteq!$F$9)","v":1.2803812195909461},""]
["TECHNIK","WR 071071",null,"Bit pro šrouby s drážkou","1ks",4.5277248924665336,{"$f":"F5741*(1-Elteq!$F$9)","v":4.5277248924665336},""]
["TECHNIK","WR 071072",null,"Bit pro šrouby s drážkou 2,5x25mm","1ks",4.5277248924665336,{"$f":"F5742*(1-Elteq!$F$9)","v":4.5277248924665336},""]
["TECHNIK","WR 071074",null,"Bit pro šrouby s drážkou 4,0x25mm","1ks",4.5277248924665336,{"$f":"F5743*(1-Elteq!$F$9)","v":4.5277248924665336},""]
["TECHNIK","WR 072050",null,"Bit WERA pro šrouby s drážkou 0,5x4,0mm - houževnatý","1ks",0.85358747972729732,{"$f":"F5744*(1-Elteq!$F$9)","v":0.85358747972729732},""]
["TECHNIK","WR 072055",null,"Bit WERA pro šrouby s drážkou 0,6x4,5mm - houževnatý","1ks",0.85358747972729732,{"$f":"F5745*(1-Elteq!$F$9)","v":0.85358747972729732},""]
["TECHNIK","WR 072057",null,"Bit WERA pro šrouby s drážkou 0,8x5,5mm - houževnatý","1ks",0.85358747972729732,{"$f":"F5746*(1-Elteq!$F$9)","v":0.85358747972729732},""]
["TECHNIK","WR 072059",null,"Bit WERA pro šrouby s drážkou 1,0x5,5mm - houževnatý","1ks",0.85358747972729732,{"$f":"F5747*(1-Elteq!$F$9)","v":0.85358747972729732},""]
["TECHNIK","WR 072061",null,"Bit WERA pro šrouby s drážkou 1,2x6,5mm - houževnatý","1ks",0.85358747972729732,{"$f":"F5748*(1-Elteq!$F$9)","v":0.85358747972729732},""]
["TECHNIK","WR 072063",null,"Bit WERA pro šrouby s drážkou 1,2x8,0mm - houževnatý","1ks",0.85358747972729732,{"$f":"F5749*(1-Elteq!$F$9)","v":0.85358747972729732},""]
["TECHNIK","WR 072065",null,"Bit WERA pro šrouby s drážkou 1,6x8,0mm - houževnatý","1ks",0.85358747972729732,{"$f":"F5750*(1-Elteq!$F$9)","v":0.85358747972729732},""]
["TECHNIK","WR 072070",null,"Bit WERA pro křížové šrouby PH 1 - standardní","1ks",0.61235623545653939,{"$f":"F5751*(1-Elteq!$F$9)","v":0.61235623545653939},""]
["TECHNIK","WR 072072",null,"Bit WERA pro křížové šrouby PH 2 - standardní","1ks",0.61235623545653939,{"$f":"F5752*(1-Elteq!$F$9)","v":0.61235623545653939},""]
["TECHNIK","WR 072074",null,"Bit WERA pro křížové šrouby PH 3 - standardní","1ks",0.61235623545653939,{"$f":"F5753*(1-Elteq!$F$9)","v":0.61235623545653939},""]
["TECHNIK","WR 072082",null,"Bit WERA pro křížové šrouby PZ 2 - standardní","1ks",0.61235623545653939,{"$f":"F5754*(1-Elteq!$F$9)","v":0.61235623545653939},""]
["TECHNIK","WR 134480",null,"Držák bitů WERA s rychloupínací hlavou a magnetem","1ks",5.8266623616167692,{"$f":"F5755*(1-Elteq!$F$9)","v":5.8266623616167692},""]
["TECHNIK","AM  1",null,"Odplášťovací nůž pro průměry 4,5-25mm / síla izolace PVC max. 4,5mm economy","1ks",13.174937187095242,{"$f":"F5756*(1-Elteq!$F$9)","v":13.174937187095242},"8591735046583"]
["TECHNIK","AM  5-28",null,"Odplášťovací nůž pro průměry 5-28mm / síla izolace PVC max. 4,5mm profi","1ks",32.658999224348769,{"$f":"F5757*(1-Elteq!$F$9)","v":32.658999224348769},"8591735009472"]
["TECHNIK","AM  8-25",null,"Odplášťovací nůž pro průměry 8-25mm / síla izolace PVC max. 4,5mm profi","1ks",65.317998448697537,{"$f":"F5758*(1-Elteq!$F$9)","v":65.317998448697537},"8591735009489"]
["TECHNIK","AM 15-36",null,"Odplášťovací nůž pro průměry 15-36mm / síla izolace PVC max. 5,0mm profi","1ks",169.23299598071634,{"$f":"F5759*(1-Elteq!$F$9)","v":169.23299598071634},"8591735009496"]
["TECHNIK","AM 20-60",null,"Odplášťovací nůž pro průměry 20-60mm / síla izolace PVC max. 5,0mm profi","1ks",200.03637024913621,{"$f":"F5760*(1-Elteq!$F$9)","v":200.03637024913621},"8591735009502"]
["TECHNIK","AM 25 H",null,"Odplášťovací nůž pro průměry 4,5-25mm / síla izolace PVC max. 4,5mm economy","1ks",25.60762439181892,{"$f":"F5761*(1-Elteq!$F$9)","v":25.60762439181892},"8591735027049"]
["TECHNIK","AM 25 P",null,"Odplášťovací nůž pro průměry 6,0-25mm / síla izolace PVC max. 4,5mm profi Weidmüller 9001540000","1ks",32.844561719941659,{"$f":"F5762*(1-Elteq!$F$9)","v":32.844561719941659},"8591735056858"]
["TECHNIK","AM 35 H",null,"Odplášťovací nůž pro průměry 10-35mm / síla izolace PVC max. 4,5mm economy","1ks",29.318874303676736,{"$f":"F5763*(1-Elteq!$F$9)","v":29.318874303676736},"8591735027995"]
["TECHNIK","AM 35 P",null,"Odplášťovací nůž pro průměry 25-36mm / síla izolace PVC max. 4,5mm profi Weidmüller 9001080000","1ks",37.669186605356821,{"$f":"F5764*(1-Elteq!$F$9)","v":37.669186605356821},"8591735056865"]
["TECHNIK","AM-K",null,"9856 KNIPEX odplášťovací nůž do 1000V, rovná čepel s krytkou","1ks",21.673699485249639,{"$f":"F5765*(1-Elteq!$F$9)","v":21.673699485249639},"8591735008932"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"AM-M",null,"Odplášťovací nůž do 1000V, čepel s vodící ploškou","1ks",10.948187239980554,{"$f":"F5766*(1-Elteq!$F$9)","v":10.948187239980554},"8591735008949"]
["TECHNIK","AM-MI",null,"9855 KNIPEX Odplášťovací nůž do 1000V, čepel s vodící ploškou","1ks",32.881674219060237,{"$f":"F5767*(1-Elteq!$F$9)","v":32.881674219060237},"8591735008956"]
["TECHNIK","AM-R",null,"9852 KNIPEX odplášťovací nůž do 1000V, rovná čepel s krytkou","1ks",12.544024702079414,{"$f":"F5768*(1-Elteq!$F$9)","v":12.544024702079414},"8591735008963"]
["TECHNIK","AM-X",null,"1640150 KNIPEX odplášťovací nůž profesionální pro průměry nad 25mm","1ks",203.97029515570549,{"$f":"F5769*(1-Elteq!$F$9)","v":203.97029515570549},"8591735008970"]
["TECHNIK","CIM 12 0500",null,"Kapesní pilka s nastavitelnou rukojetí","1ks",10.539949749676193,{"$f":"F5770*(1-Elteq!$F$9)","v":10.539949749676193},""]
["TECHNIK","COAX-STRIP  8",null,"Nůž k odizolování koaxiálních kabelů RG 58/59/62/6 se třemi nastavitelnými břity, rozteč 8/4mm","1ks",9.3894622770002716,{"$f":"F5771*(1-Elteq!$F$9)","v":9.3894622770002716},"8591735009342"]
["TECHNIK","COAX-STRIP 12",null,"Nůž k odizolování koaxiálních kabelů RG 213 se dvěma hloubkově nastavitelnými břity, rozteč 8mm","1ks",9.3894622770002716,{"$f":"F5772*(1-Elteq!$F$9)","v":9.3894622770002716},"8591735019501"]
["TECHNIK","COAX-STRIP 12/3",null,"Nůž k odizolování koaxiálních kabelů RG 8/11/213 se dvěma pevně uloženými břity, rozteč 3,18mm","1ks",8.3503123016800824,{"$f":"F5773*(1-Elteq!$F$9)","v":8.3503123016800824},"8591735028008"]
["TECHNIK","COAX-STRIP 12/6",null,"Nůž k odizolování koaxiálních kabelů RG 8/11/213 se dvěma pevně uloženými břity, rozteč 6,35mm","1ks",8.3503123016800824,{"$f":"F5774*(1-Elteq!$F$9)","v":8.3503123016800824},"8591735028015"]
["TECHNIK","COAX-STRIP UNI",null,"Nůž k odizolování koaxiálních kabelů RG 174/158/59/62/6 se dvěma nastavit. břity, rozteč 4/6/8/12mm","1ks",9.0925622840516453,{"$f":"F5775*(1-Elteq!$F$9)","v":9.0925622840516453},"8591735052010"]
["TECHNIK","COSSONAY I",null,"Odplášťovací nůž, neizolovaná čepel s vodící ploškou","1ks",73.482748254784724,{"$f":"F5776*(1-Elteq!$F$9)","v":73.482748254784724},"8591735028022"]
["TECHNIK","COSSONAY II",null,"Odplášťovací nůž, izolovaná čepel s vodící ploškou","1ks",77.936248149014105,{"$f":"F5777*(1-Elteq!$F$9)","v":77.936248149014105},"8591735047542"]
["TECHNIK","Čepel A",null,"Náhradní karbonová čepel vypichovací","5ks",7.4596123228342073,{"$f":"F5778*(1-Elteq!$F$9)","v":7.4596123228342073},"8591735028039"]
["TECHNIK","Čepel H",null,"Náhradní karbonová čepel háčková","10ks",4.6761748889408468,{"$f":"F5779*(1-Elteq!$F$9)","v":4.6761748889408468},"8591735028046"]
["TECHNIK","Čepel L",null,"Náhradní karbonová čepel na lino","5ks",7.4596123228342073,{"$f":"F5780*(1-Elteq!$F$9)","v":7.4596123228342073},"8591735028053"]
["TECHNIK","Čepel ODL  9",null,"Náhradní karbonová čepel odlamovací 9mm","10ks",2.2267499471146888,{"$f":"F5781*(1-Elteq!$F$9)","v":2.2267499471146888},"8591735028060"]
["TECHNIK","Čepel ODL 18",null,"Náhradní karbonová čepel odlamovací 18mm (CB18)","10ks",3.1545624250791424,{"$f":"F5782*(1-Elteq!$F$9)","v":3.1545624250791424},"8591735028077"]
["TECHNIK","Čepel ODL-BM 18",null,"Náhradní bimetalová čepel odlamovací 18mm","5ks",3.4514624180277678,{"$f":"F5783*(1-Elteq!$F$9)","v":3.4514624180277678},"8591735028084"]
["TECHNIK","Čepel ODL-BM 18/50",null,"Náhradní bimetalová čepel odlamovací 18mm","50ks",32.102311737570098,{"$f":"F5784*(1-Elteq!$F$9)","v":32.102311737570098},"8591735028091"]
["TECHNIK","Čepel T",null,"Náhradní karbonová čepel trapézová","10ks",3.3772374197906112,{"$f":"F5785*(1-Elteq!$F$9)","v":3.3772374197906112},"8591735028107"]
["TECHNIK","Čepel T-BM",null,"Náhradní bimetalová čepel trapézová","10ks",6.4946873457511751,{"$f":"F5786*(1-Elteq!$F$9)","v":6.4946873457511751},"8591735028114"]
["TECHNIK","DATA-STRIP",null,"Nůž k odizolování datových kabelů o průměru 2-10mm","1ks",13.249162185332398,{"$f":"F5787*(1-Elteq!$F$9)","v":13.249162185332398},"8591735009359"]
["TECHNIK","DBKPH-SET",null,"Univerzální zavírací nůž s výměnnými čepelemi","1sada",26.164311878597594,{"$f":"F5788*(1-Elteq!$F$9)","v":26.164311878597594},"8591735028121"]
["TECHNIK","DMT-SET",null,"Univerzální zavírací nůž s LED svítilnou a průmyslovými nůžkami v sadě","1sada",32.06519923845152,{"$f":"F5789*(1-Elteq!$F$9)","v":32.06519923845152},""]
["TECHNIK","JOKARI 10280",null,"Odizolovací nůž pro průměry vodičů 8-28mm s pevným břitem ve tvaru háku JOKARI Secura","1ks",15.179012139498461,{"$f":"F5790*(1-Elteq!$F$9)","v":15.179012139498461},"8591735050993"]
["TECHNIK","JOKARI 10282",null,"Odizolovací nůž pro průměry vodičů 8-28mm s pevným břitem ve tvaru háku JOKARI","1ks",9.8348122664232083,{"$f":"F5791*(1-Elteq!$F$9)","v":9.8348122664232083},"8591735051532"]
["TECHNIK","JOKARI 30010",null,"Odizolovací nůž JOKARI pro koaxiální kabely RG 58 a RG 59","1ks",16.997524596308789,{"$f":"F5792*(1-Elteq!$F$9)","v":16.997524596308789},""]
["TECHNIK","JOKARI 30140",null,"Odizolovací nůž pro ploché a oválné kabely do šíře 12mm JOKARI No.14","1ks",32.473436728755878,{"$f":"F5793*(1-Elteq!$F$9)","v":32.473436728755878},""]
["TECHNIK","JOKARI 30155",null,"Odizolovací nůž pro průměry kabelů 8-13mm JOKARI Secura No.15","1ks",35.331099160886396,{"$f":"F5794*(1-Elteq!$F$9)","v":35.331099160886396},""]
["TECHNIK","JOKARI ESD PLUS 001",null,"Odizolovací nůž pro průměry vodičů 0,12-0,4mm JOKARI mikro","1ks",34.514624180277679,{"$f":"F5795*(1-Elteq!$F$9)","v":34.514624180277679},""]
["TECHNIK","Nůž ML 18",null,"Nůž odlamovací Edding ML18","1ks",9.1667872822888015,{"$f":"F5796*(1-Elteq!$F$9)","v":9.1667872822888015},"4004764083039"]
["TECHNIK","Nůž MP 9",null,"Nůž odlamovací Edding MP9","1ks",7.6080623193085195,{"$f":"F5797*(1-Elteq!$F$9)","v":7.6080623193085195},""]
["TECHNIK","Nůž PE  9",null,"Nůž odlamovací ProEntry velikost 9mm","1ks",1.5587249629802822,{"$f":"F5798*(1-Elteq!$F$9)","v":1.5587249629802822},"8591735028138"]
["TECHNIK","Nůž PE 18",null,"Nůž odlamovací ProEntry velikost 18mm","1ks",2.1896374479961107,{"$f":"F5799*(1-Elteq!$F$9)","v":2.1896374479961107},"8591735028145"]
["TECHNIK","Nůž PT  9",null,"Nůž odlamovací ProTouch velikost 9mm","1ks",8.7214372928658648,{"$f":"F5800*(1-Elteq!$F$9)","v":8.7214372928658648},"8591735028152"]
["TECHNIK","Nůž PT 18",null,"Nůž odlamovací ProTouch","1ks",12.469799703842257,{"$f":"F5801*(1-Elteq!$F$9)","v":12.469799703842257},""]
["TECHNIK","Nůž PT 18 EXTREM",null,"Nůž odlamovací ProTouch EX se šroubem","1ks",11.764662220589273,{"$f":"F5802*(1-Elteq!$F$9)","v":11.764662220589273},"8591735028169"]
["TECHNIK","Nůž PT-V",null,"Nůž s vysouvací čepelí ProTouch","1ks",18.370687063696181,{"$f":"F5803*(1-Elteq!$F$9)","v":18.370687063696181},"8591735027988"]
["TECHNIK","Nůž ST  9",null,"Nůž odlamovací Standard velikost 9mm","1ks",6.1977873528025507,{"$f":"F5804*(1-Elteq!$F$9)","v":6.1977873528025507},"8591735028176"]
["TECHNIK","Nůž ST 18",null,"Nůž odlamovací Standard velikost 18mm","1ks",7.3853873245970512,{"$f":"F5805*(1-Elteq!$F$9)","v":7.3853873245970512},"8591735028183"]
["TECHNIK","Nůž ST-V",null,"Nůž s vysouvací čepelí Standard","1ks",10.354387254083303,{"$f":"F5806*(1-Elteq!$F$9)","v":10.354387254083303},"8591735028190"]
["TECHNIK","S 4-28 Voltage",null,"Odizolovací nůž pro průměry vodičů 4-28mm WE4-28S vč. bezkontaktní detekce napětí 50-600V","1ks",30.432249277234078,{"$f":"F5807*(1-Elteq!$F$9)","v":30.432249277234078},"8591735052881"]
["TECHNIK","S 4-28H",null,"Odizolovací nůž pro průměry vodičů 4-28mm WE4-28S","1ks",20.597437010810872,{"$f":"F5808*(1-Elteq!$F$9)","v":20.597437010810872},"8591735028206"]
["TECHNIK","STRIPIT 12",null,"Nůž k odizolování datových kabelů o průměru 3-12mm (AM 12)","1ks",27.092124356562046,{"$f":"F5809*(1-Elteq!$F$9)","v":27.092124356562046},"8591735018351"]
["TECHNIK","WE 13",null,"Odizolovací nůž pro AL a CU vodiče o průměru 8-13mm","1ks",16.700624603360165,{"$f":"F5810*(1-Elteq!$F$9)","v":16.700624603360165},"8591735028237"]
["TECHNIK","WE 2",null,"Odizolovací nůž pro koaxiální vodiče o průměru 4,8-7,5mm","1ks",16.329499612174384,{"$f":"F5811*(1-Elteq!$F$9)","v":16.329499612174384},"8591735028213"]
["TECHNIK","WE 28-35",null,"Odizolovací nůž pro průměry vodičů 28-35mm","1ks",16.143937116581494,{"$f":"F5812*(1-Elteq!$F$9)","v":16.143937116581494},"8591735009007"]
["TECHNIK","WE 3",null,"Odizolovací nůž pro koaxiální vodiče 4,8-7,5mm s integrovanými břity pro střihání vodičů","1ks",16.143937116581494,{"$f":"F5813*(1-Elteq!$F$9)","v":16.143937116581494},"8591735038151"]
["TECHNIK","WE 35-50",null,"Odizolovací nůž pro průměry vodičů 35-50mm","1ks",16.143937116581494,{"$f":"F5814*(1-Elteq!$F$9)","v":16.143937116581494},"8591735009014"]
["TECHNIK","WE 4-16",null,"Odizolovací nůž pro průměry vodičů 4-16mm","1ks",10.948187239980554,{"$f":"F5815*(1-Elteq!$F$9)","v":10.948187239980554},"8591735038144"]
["TECHNIK","WE 4-28G",null,"Odizolovací nůž pro průměry vodičů 4-28mm s pevným rovným břitem","1ks",12.247124709130787,{"$f":"F5816*(1-Elteq!$F$9)","v":12.247124709130787},"8591735038090"]
["TECHNIK","WE 4-28H",null,"Odizolovací nůž pro průměry vodičů 4-28mm s pevným břitem ve tvaru háku","1ks",12.247124709130787,{"$f":"F5817*(1-Elteq!$F$9)","v":12.247124709130787},"8591735008987"]
["TECHNIK","WE 8-27",null,"Odizolovací nůž pro průměry vodičů 8-27mm","1ks",10.948187239980554,{"$f":"F5818*(1-Elteq!$F$9)","v":10.948187239980554},"8591735008994"]
["TECHNIK","WE100",null,"Odizolovací nůž pro průměry vodičů 4-13mm a vnitřní izolace vodičů 0,5-16mm2","1ks",17.925337074273244,{"$f":"F5819*(1-Elteq!$F$9)","v":17.925337074273244},"8591735028220"]
["TECHNIK","WE400",null,"Odizolovací nůž pro průměry vodičů 8-13mm s funkcí stříhání do 6mm2 laněné, do 4mm2 plné vodiče","1ks",26.349874374190485,{"$f":"F5820*(1-Elteq!$F$9)","v":26.349874374190485},"8591735028244"]
["TECHNIK","WE500",null,"Multifunkční odizolovací nůž se zkoušečkou a šroubováky","1ks",58.823311102946363,{"$f":"F5821*(1-Elteq!$F$9)","v":58.823311102946363},"8591735028251"]
["TECHNIK","KS 160/1000",null,"Kleště štípací stranové 160mm do 1000V","1ks",17.851112076036088,{"$f":"F5822*(1-Elteq!$F$9)","v":17.851112076036088},"8591735013165"]
["TECHNIK","PN  1",null,"Nůžky na Al a Cu vodiče do průměru 1,6mm, černěné, masivní rukojeti","1ks",14.288312160652586,{"$f":"F5823*(1-Elteq!$F$9)","v":14.288312160652586},"8591735011048"]
["TECHNIK","PN  8",null,"Nůžky na Al a Cu vodiče do průměru 8mm vhodné pro plný drát, masivní rukojeti","1ks",33.77237419790611,{"$f":"F5824*(1-Elteq!$F$9)","v":33.77237419790611},"8591735011673"]
["TECHNIK","PN  8/1",null,"Nůžky na Al a Cu vodiče do průměru 8mm vhodné pro plný drát, potahované rukojeti","1ks",33.030124215534549,{"$f":"F5825*(1-Elteq!$F$9)","v":33.030124215534549},"8591735042462"]
["TECHNIK","PN 12",null,"Nůžky na Al a Cu vodiče do průměru 12mm, délka 160mm","1ks",15.698587127158556,{"$f":"F5826*(1-Elteq!$F$9)","v":15.698587127158556},"8591735007676"]
["TECHNIK","PN 14K",null,"Pákové nůžky na Al a Cu kabely do průměru 14mm, délka 300mm, hmotnost 0,7kg (K100)","1ks",28.79929931601664,{"$f":"F5827*(1-Elteq!$F$9)","v":28.79929931601664},"8591735036430"]
["TECHNIK","PN 16",null,"Nůžky na Al a Cu vodiče do průměru 16mm, masivní rukojeti  (PN15)","1ks",28.576624321305172,{"$f":"F5828*(1-Elteq!$F$9)","v":28.576624321305172},"8591735009021"]
["TECHNIK","PN 16/1",null,"9511165 KNIPEX nůžky na Al a Cu vodiče do průměru 16mm, potahované rukojeti (PN15/1)","1ks",22.638624462332668,{"$f":"F5829*(1-Elteq!$F$9)","v":22.638624462332668},"8591735009038"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"PN 16/1 STRIP",null,"Nůžky na Al a Cu vodiče do průměru 16mm s odizolováním 1,5-2,5mm2, potahované rukojeti","1ks",36.926936622985252,{"$f":"F5830*(1-Elteq!$F$9)","v":36.926936622985252},"8591735052829"]
["TECHNIK","PN 16/1000",null,"9516165 KNIPEX nůžky do 1000V na Al a Cu vodiče do průměru 16mm, dvoukomponentní rukojeti","1ks",41.046424025147431,{"$f":"F5831*(1-Elteq!$F$9)","v":41.046424025147431},"8591735009045"]
["TECHNIK","PN 16/1P",null,"9521165 KNIPEX nůžky na Al a Cu vodiče do průměru 16mm, potahované rukojeti s vratnou pružinou","1ks",29.689999294862517,{"$f":"F5832*(1-Elteq!$F$9)","v":29.689999294862517},"8591735035600"]
["TECHNIK","PN 16/P",null,"Nůžky na Al a Cu vodiče do pruměru 16mm, masivní rukojeti s vratnou průžinou","1ks",32.287874233162988,{"$f":"F5833*(1-Elteq!$F$9)","v":32.287874233162988},"8591735048013"]
["TECHNIK","PN 24",null,"Silové nůžky na Al a Cu vodiče do průřezu 60mm2, potahované rukojeti","1ks",35.924899146783645,{"$f":"F5834*(1-Elteq!$F$9)","v":35.924899146783645},"8591735050528"]
["TECHNIK","PN 25",null,"Nůžky na Al a Cu vodiče do průměru 25mm, masivní rukojeti (PN20)","1ks",48.617373845337369,{"$f":"F5835*(1-Elteq!$F$9)","v":48.617373845337369},"8591735009052"]
["TECHNIK","PN 25/1",null,"9511200 KNIPEX nůžky na Al a Cu vodiče do průměru 25mm, potahované rukojeti (PN20/1)","1ks",39.895936552471504,{"$f":"F5836*(1-Elteq!$F$9)","v":39.895936552471504},"8591735009069"]
["TECHNIK","PN 25/1000",null,"9516200 KNIPEX nůžky do 1000V na Al a Cu vodiče do průměru 25mm, dvoukomponentní rukojeti","1ks",52.291511258076611,{"$f":"F5837*(1-Elteq!$F$9)","v":52.291511258076611},"8591735009076"]
["TECHNIK","PN 26T",null,"Pákové nůžky na Al a Cu kabely s teleskopickými rukojeťmi do průměru 26mm (K105/1) originál Klauke","1ks",188.53149552237699,{"$f":"F5838*(1-Elteq!$F$9)","v":188.53149552237699},"8591735011680"]
["TECHNIK","PN 26TL",null,"Pákové nůžky na Al a Cu kabely s teleskopickými rukojeťmi do průměru 26mm (K105/1) červené rukojeti","1ks",131.74937187095242,{"$f":"F5839*(1-Elteq!$F$9)","v":131.74937187095242},"8591735050801"]
["TECHNIK","PN 27",null,"9512500 KNIPEX pákové nůžky na Al a Cu kabely do průměru 27mm, délka 500mm, hmotnost 1,1kg","1ks",96.121372717117396,{"$f":"F5840*(1-Elteq!$F$9)","v":96.121372717117396},"8591735010706"]
["TECHNIK","PN 27/1000",null,"9517500 KNIPEX pákové nůžky do 1000V na Al a Cu kabely do průměru 27mm","1ks",136.09153426782606,{"$f":"F5841*(1-Elteq!$F$9)","v":136.09153426782606},"8591735045524"]
["TECHNIK","PN 30",null,"Pákové nůžky na Al a Cu kabely do průměru 30mm, délka 600mm, hmotnost 2,1kg","1ks",58.266623616167692,{"$f":"F5842*(1-Elteq!$F$9)","v":58.266623616167692},"8591735047207"]
["TECHNIK","PN 30K",null,"Pákové nůžky na Al a Cu kabely do průměru 30mm, délka 530mm, hmotnost 1,2kg (K130)","1ks",116.53324723233538,{"$f":"F5843*(1-Elteq!$F$9)","v":116.53324723233538},"8591735047221"]
["TECHNIK","PN 48",null,"9505140 KNIPEX nůžky universální ke všeobecnému použití do 48mm","1ks",15.587249629802821,{"$f":"F5844*(1-Elteq!$F$9)","v":15.587249629802821},"8591735036423"]
["TECHNIK","PN 50",null,"Pákové nůžky na Al a Cu kabely do průměru 50mm, délka 800mm, hmotnost 3,2kg","1ks",70.513748325298479,{"$f":"F5845*(1-Elteq!$F$9)","v":70.513748325298479},"8591735047238"]
["TECHNIK","PN 50K",null,"Pákové nůžky na Al a Cu kabely do průměru 50mm, délka 770mm, hmotnost 3,0kg (K150)","1ks",141.76974663296852,{"$f":"F5846*(1-Elteq!$F$9)","v":141.76974663296852},"8591735047245"]
["TECHNIK","PN 56P",null,"9415215 KNIPEX nůžky na ploché kabely do celkové šíře 56mm, délka 215mm","1ks",53.033761240448172,{"$f":"F5847*(1-Elteq!$F$9)","v":53.033761240448172},"8591735046071"]
["TECHNIK","PN DATA",null,"Nůžky na datové vodiče","1ks",58.266623616167692,{"$f":"F5848*(1-Elteq!$F$9)","v":58.266623616167692},"8591735035273"]
["TECHNIK","PN OPTI",null,"Nůžky na optické vodiče","1ks",42.679373986364865,{"$f":"F5849*(1-Elteq!$F$9)","v":42.679373986364865},"8591735035280"]
["TECHNIK","PNFE  3/5",null,"9561190 KNIPEX pákové nůžky na Fe dráty do průměru 3mm a lana do 5mm, délka 190mm (PN46)","1ks",44.906123933479556,{"$f":"F5850*(1-Elteq!$F$9)","v":44.906123933479556},"8591735009571"]
["TECHNIK","PNFE  4-6",null,"7101200 KNIPEX pákové nůžky na Fe dráty do průměru 4-6mm, potahované rukojeti, (PN36)","1ks",33.475474204957486,{"$f":"F5851*(1-Elteq!$F$9)","v":33.475474204957486},"8591735009588"]
["TECHNIK","PNFE  4-6 P",null,"7112200 KNIPEX pákové nůžky na Fe dráty do průměru 4-6mm, masivní rukojeti, vratná pružina (PN36/1)","1ks",40.118611547182972,{"$f":"F5852*(1-Elteq!$F$9)","v":40.118611547182972},"8591735047191"]
["TECHNIK","PNFE  5/7",null,"Pákové nůžky na Fe dráty do průměru 5mm a lana do 7mm, délka 310mm, hmotnost 0,7kg (PN57)","1ks",91.036960337872188,{"$f":"F5853*(1-Elteq!$F$9)","v":91.036960337872188},"8591735048846"]
["TECHNIK","PNFE  7/10",null,"Pákové nůžky na Fe dráty do průměru 7mm a lana do 10mm, délka 445mm, hmotnost 1,1kg (PN710)","1ks",95.935810221524505,{"$f":"F5854*(1-Elteq!$F$9)","v":95.935810221524505},"8591735048839"]
["TECHNIK","PNFE  9/12",null,"Pákové nůžky na Fe dráty do průměru 9mm a lana do 14mm, délka 600mm, hmotnost 2,1kg (PN912)","1ks",89.404010376654753,{"$f":"F5855*(1-Elteq!$F$9)","v":89.404010376654753},"8591735009649"]
["TECHNIK","PNFE 11/16",null,"Pákové nůžky na Fe dráty do průměru 11mm a lana do 16mm, délka 600mm, hmotnost 2,1kg (PN1116)","1ks",239.22716931835473,{"$f":"F5856*(1-Elteq!$F$9)","v":239.22716931835473},"8591735050177"]
["TECHNIK","PNFE 40x4",null,"Pákové nůžky na plochou ocel do 40x4mm, délka 840mm","1ks",245.68474416498734,{"$f":"F5857*(1-Elteq!$F$9)","v":245.68474416498734},"8591735009564"]
["TECHNIK","PNFE B  4/6",null,"Pákové nůžky na Fe dráty do 5mm a lana do 6mm, délka 350mm, Baudat","1ks",97.234747690674737,{"$f":"F5858*(1-Elteq!$F$9)","v":97.234747690674737},""]
["TECHNIK","PNFE B  7/10",null,"Pákové nůžky na Fe dráty do 6mm a lana do 10mm, délka 500mm, Baudat","1ks",172.38755840579549,{"$f":"F5859*(1-Elteq!$F$9)","v":172.38755840579549},"8591735009618"]
["TECHNIK","PNFE B 10/14",null,"Pákové nůžky na Fe dráty do 8mm a lana do 14mm, délka 720mm, Baudat","1ks",237.33443186330723,{"$f":"F5860*(1-Elteq!$F$9)","v":237.33443186330723},"8591735009557"]
["TECHNIK","PNFE U  5-8",null,"7172460 KNIPEX pákové nůžky na Fe dráty a svorníky do průměru 5-8mm, délka 460mm","1ks",82.872210531785001,{"$f":"F5861*(1-Elteq!$F$9)","v":82.872210531785001},""]
["TECHNIK","PNFE U  7-9",null,"7172610 KNIPEX pákové nůžky na Fe dráty a svorníky do průměru 7-9mm, délka 610mm","1ks",97.717210179216252,{"$f":"F5862*(1-Elteq!$F$9)","v":97.717210179216252},""]
["TECHNIK","PNFE U  8-11",null,"7172760 KNIPEX pákové nůžky na Fe dráty a svorníky do průměru 8-11mm, délka 760mm","1ks",127.92678446173886,{"$f":"F5863*(1-Elteq!$F$9)","v":127.92678446173886},""]
["TECHNIK","PNFE U  9-13",null,"7172910 KNIPEX pákové nůžky na Fe dráty a svorníky do průměru 9-13mm, délka 910mm","1ks",176.02458331941614,{"$f":"F5864*(1-Elteq!$F$9)","v":176.02458331941614},""]
["TECHNIK","PNFE. 4-5",null,"Pákové nůžky na Fe dráty a svorníky do průměru 4-5mm, délka 300mm","1ks",48.580261346218791,{"$f":"F5865*(1-Elteq!$F$9)","v":48.580261346218791},"8591735052706"]
["TECHNIK","PNFE. 5-7",null,"Pákové nůžky na Fe dráty a svorníky do průměru 5-7mm, délka 350mm","1ks",51.21524878363784,{"$f":"F5866*(1-Elteq!$F$9)","v":51.21524878363784},"8591735009595"]
["TECHNIK","PNFE. 6-8",null,"Pákové nůžky na Fe dráty a svorníky do průměru 6-8mm, délka 450mm","1ks",66.542710919610613,{"$f":"F5867*(1-Elteq!$F$9)","v":66.542710919610613},"8591735009601"]
["TECHNIK","PNFE. 8-10",null,"Pákové nůžky na Fe dráty a svorníky do průměru 8-10mm, délka 600mm","1ks",89.218447881061863,{"$f":"F5868*(1-Elteq!$F$9)","v":89.218447881061863},"8591735009625"]
["TECHNIK","PNFE.10-13",null,"Pákové nůžky na Fe dráty a svorníky do průměru 10-13mm, délka 750mm","1ks",121.2465346203948,{"$f":"F5869*(1-Elteq!$F$9)","v":121.2465346203948},"8591735009632"]
["TECHNIK","PNFE.11-16",null,"Pákové nůžky na Fe dráty a svorníky do průměru 11-16mm, délka 900mm","1ks",170.04947096132506,{"$f":"F5870*(1-Elteq!$F$9)","v":170.04947096132506},"8591735009656"]
["TECHNIK","PNFE.13-18",null,"Pákové nůžky na Fe dráty a svorníky do průměru 13-18mm, délka 1050mm","1ks",220.04000727404983,{"$f":"F5871*(1-Elteq!$F$9)","v":220.04000727404983},"8591735052713"]
["TECHNIK","RN 25 F",null,"Ráčnové nůžky na AL a CU kabely do průměru 25mm, verze PROFI","1ks",206.53105759488739,{"$f":"F5872*(1-Elteq!$F$9)","v":206.53105759488739},"8591735052454"]
["TECHNIK","RN 32",null,"Ráčnové nůžky na AL a CU kabely do průměru 32mm, verze ECONOMY","1ks",110.2241223821771,{"$f":"F5873*(1-Elteq!$F$9)","v":110.2241223821771},"8591735009663"]
["TECHNIK","RN 32 KN",null,"9531250 KNIPEX ráčnové nůžky na AL a CU kabely do průměru 32mm","1ks",193.69013289985935,{"$f":"F5874*(1-Elteq!$F$9)","v":193.69013289985935},"8591735032975"]
["TECHNIK","RN 32 KN/1000",null,"9536250 KNIPEX ráčnové nůžky na AL a CU kabely do průměru 32mm, izolované do 1000V","1ks",217.29368233927505,{"$f":"F5875*(1-Elteq!$F$9)","v":217.29368233927505},"8591735009670"]
["TECHNIK","RN 33",null,"Ráčnové nůžky na AL a CU kabely do průměru 32mm, délka 240mm, hmotnost 0,6kg","1ks",131.74937187095242,{"$f":"F5876*(1-Elteq!$F$9)","v":131.74937187095242},"8591735051518"]
["TECHNIK","RN 34",null,"Ráčnové nůžky na AL a CU kabely do průměru 32mm, verze PROFI (K106/1)","1ks",164.03724610411541,{"$f":"F5877*(1-Elteq!$F$9)","v":164.03724610411541},"8591735032999"]
["TECHNIK","RN 34 F",null,"Ráčnové nůžky na AL a CU kabely do průměru 34mm, verze PROFI","1ks",229.28101955457578,{"$f":"F5878*(1-Elteq!$F$9)","v":229.28101955457578},"8591735033002"]
["TECHNIK","RN 34 M",null,"Ráčnové nůžky na AL a CU kabely do průměru 35mm, masivní provedení (RN34R)","1ks",155.50137130684243,{"$f":"F5879*(1-Elteq!$F$9)","v":155.50137130684243},"8591735033019"]
["TECHNIK","RN 35 P",null,"Ráčnové nůžky na AL a CU kabely do průměru 35mm, verze PROFI","1ks",225.79244463742944,{"$f":"F5880*(1-Elteq!$F$9)","v":225.79244463742944},"8591735033026"]
["TECHNIK","RN 38 T",null,"9532038 KNIPEX ráčnové nůžky teleskopické na kabely do průměru 38mm (PN38T)","1ks",209.68562001996654,{"$f":"F5881*(1-Elteq!$F$9)","v":209.68562001996654},"8591735033828"]
["TECHNIK","RN 40 PB",null,"Ráčnové nůžky na AL a CU kabely do průměru 40mm, připojitelné na vrtačku (akkušroubovák)","1ks",777.69241902980502,{"$f":"F5882*(1-Elteq!$F$9)","v":777.69241902980502},"8591735021061"]
["TECHNIK","RN 42 M",null,"Ráčnové nůžky na AL a CU kabely do průměru 42mm, masivní provedení","1ks",148.26443397871969,{"$f":"F5883*(1-Elteq!$F$9)","v":148.26443397871969},"8591735055783"]
["TECHNIK","RN 45 P",null,"Ráčnové nůžky na AL a CU kabely do průměru 45mm, verze PROFI","1ks",287.91876816192928,{"$f":"F5884*(1-Elteq!$F$9)","v":287.91876816192928},"8591735033033"]
["TECHNIK","RN 50 UNI SET",null,"Ráčnové nůžky na kabely do průměru 50mm, s výměnnými čelistmi","1ks",526.99748748380966,{"$f":"F5885*(1-Elteq!$F$9)","v":526.99748748380966},"8591735027001"]
["TECHNIK","RN 52",null,"Ráčnové nůžky na AL a CU kabely do průměru 52mm, verze ECONOMY","1ks",140.65637165941118,{"$f":"F5886*(1-Elteq!$F$9)","v":140.65637165941118},"8591735017897"]
["TECHNIK","RN 52 KN",null,"9531280 KNIPEX ráčnové nůžky na AL a CU kabely do prům. 52mm, síla nožů 6,1mm / délka 280mm / 0,9kg","1ks",259.78749383004703,{"$f":"F5887*(1-Elteq!$F$9)","v":259.78749383004703},"8591735033040"]
["TECHNIK","RN 52 KN/1000",null,"9536280 KNIPEX ráčnové nůžky na AL a CU kabely do průměru 52mm, izolované do 1000V","1ks",288.73524314253797,{"$f":"F5888*(1-Elteq!$F$9)","v":288.73524314253797},"8591735047436"]
["TECHNIK","RN 52 M",null,"Ráčnové nůžky na AL a CU kabely do prům. 52mm, síla nožů 7,5mm / délka 320mm / 1,0kg masivní","1ks",304.87918025911949,{"$f":"F5889*(1-Elteq!$F$9)","v":304.87918025911949},"8591735033057"]
["TECHNIK","RN 52 P",null,"Ráčnové nůžky na AL a CU kabely do průměru 52mm, síla nožů 8,5mm / délka 325mm / 1,2kg PROFI (RN52R)","1ks",356.2799915383502,{"$f":"F5890*(1-Elteq!$F$9)","v":356.2799915383502},"8591735033064"]
["TECHNIK","RN 52/1000",null,"Ráčnové nůžky na AL a CU kabely do průměru 52mm, izolované do 1000V","1ks",244.94249418261577,{"$f":"F5891*(1-Elteq!$F$9)","v":244.94249418261577},"8591735009694"]
["TECHNIK","RN 53",null,"Ráčnové nůžky na AL a CU kabely do průměru 52mm, síla nožů 5,9mm / délka 260mm / hmotnost 0,9kg","1ks",158.84149622751445,{"$f":"F5892*(1-Elteq!$F$9)","v":158.84149622751445},"8591735033071"]
["TECHNIK","RN 54",null,"Ráčnové nůžky na AL a CU kabely do průměru 54mm, délka 310mm, hmotnost 0,84kg, verze PROFI (K106/2)","1ks",277.23036841577874,{"$f":"F5893*(1-Elteq!$F$9)","v":277.23036841577874},"8591735009687"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"RN 55",null,"Ráčnové nůžky na AL a CU kabely do průměru 55mm, délka 430mm","1ks",204.86099513455136,{"$f":"F5894*(1-Elteq!$F$9)","v":204.86099513455136},"8591735017903"]
["TECHNIK","RN 60",null,"Ráčnové nůžky na AL a CU kabely do průměru 60mm, délka 720mm, hmotnost 4,8kg (K103/1)","1ks",569.67686147017457,{"$f":"F5895*(1-Elteq!$F$9)","v":569.67686147017457},"8591735009700"]
["TECHNIK","RN 60 KN",null,"9532320 KNIPEX ráčnové nůžky na AL a CU kabely do průměru 60mm","1ks",320.87466737922665,{"$f":"F5896*(1-Elteq!$F$9)","v":320.87466737922665},"8591735047900"]
["TECHNIK","RN 60 KN/1000",null,"9536320 KNIPEX ráčnové nůžky na AL a CU kabely do průměru 60mm, izolované do 1000V","1ks",349.19150420670178,{"$f":"F5897*(1-Elteq!$F$9)","v":349.19150420670178},"8591735047917"]
["TECHNIK","RN 60T",null,"9532060 KNIPEX ráčnové nůžky s teleskopickými rukojeťmi na AL a CU kabely do průměru 60mm","1ks",611.24286048298211,{"$f":"F5898*(1-Elteq!$F$9)","v":611.24286048298211},"8591735033835"]
["TECHNIK","RN 62 P",null,"Ráčnové nůžky na AL a CU kabely do průměru 62mm","1ks",591.94436094132141,{"$f":"F5899*(1-Elteq!$F$9)","v":591.94436094132141},"8591735033101"]
["TECHNIK","RN 62 S",null,"Ráčnové nůžky zesílené na AL a CU kabely do průměru 62mm","1ks",599.36686076503702,{"$f":"F5900*(1-Elteq!$F$9)","v":599.36686076503702},"8591735033118"]
["TECHNIK","RN 65",null,"Ráčnové nůžky na AL a CU kabely do průměru 65mm, délka 550mm, hmotnost 3,5kg","1ks",476.8956136737292,{"$f":"F5901*(1-Elteq!$F$9)","v":476.8956136737292},"8591735051525"]
["TECHNIK","RN 80 S",null,"Ráčnové nůžky zesílené na AL a CU kabely do průměru 80mm","1ks",666.16935917847775,{"$f":"F5902*(1-Elteq!$F$9)","v":666.16935917847775},"8591735033125"]
["TECHNIK","RN 85 PB",null,"Ráčnové nůžky na AL a CU kabely do průměru 89mm, připojitelné na vrtačku (akkušroubovák)","1ks",1105.0246612556643,{"$f":"F5903*(1-Elteq!$F$9)","v":1105.0246612556643},"8591735053666"]
["TECHNIK","RN 92",null,"Ráčnové nůžky na AL a CU kabely do průměru 92mm, délka 630mm, BAUDAT HC92","1ks",611.98511046535361,{"$f":"F5904*(1-Elteq!$F$9)","v":611.98511046535361},"8591735033132"]
["TECHNIK","RN100",null,"Ráčnové nůžky na AL a CU kabely do průměru 100mm, délka 820mm, hmotnost 6,2kg (K104/1)","1ks",671.73623404626449,{"$f":"F5905*(1-Elteq!$F$9)","v":671.73623404626449},"8591735009717"]
["TECHNIK","RN100T",null,"9532100 KNIPEX ráčnové nůžky s teleskopickými rukojeťmi na kabely do průměru 100mm","1ks",708.84873316484254,{"$f":"F5906*(1-Elteq!$F$9)","v":708.84873316484254},"8591735033842"]
["TECHNIK","M 42",null,"Nůžky na plasty do šíře nebo průměru 42mm, economy (L-42W)","1ks",20.040749524032197,{"$f":"F5907*(1-Elteq!$F$9)","v":20.040749524032197},"8591735017286"]
["TECHNIK","M 42 A",null,"Nůžky na plasty do šíře nebo průměru 42mm s nožem ve tvaru \"V\", 12V","1ks",204.48987014336558,{"$f":"F5908*(1-Elteq!$F$9)","v":204.48987014336558},"8591735038779"]
["TECHNIK","M 42 P",null,"Nůžky na plasty do šíře nebo průměru 42mm s nožem ve tvaru \"V\", profi","1ks",80.534123087314583,{"$f":"F5909*(1-Elteq!$F$9)","v":80.534123087314583},"8591735038755"]
["TECHNIK","VK 16",null,"Vystřihovací kleště na plastové kanály, šíře čelistí 16mm","1ks",38.596999083321272,{"$f":"F5910*(1-Elteq!$F$9)","v":38.596999083321272},"8591735035563"]
["TECHNIK","VK 16 DL",null,"Vystřihovací kleště na plastové kanály, šíře čelistí 16mm, dlouhé rukojeti","1ks",46.019498907036898,{"$f":"F5911*(1-Elteq!$F$9)","v":46.019498907036898},"8591735051341"]
["TECHNIK","VK 20",null,"Vystřihovací kleště na plastové kanály, šíře čelistí 20mm","1ks",38.596999083321272,{"$f":"F5912*(1-Elteq!$F$9)","v":38.596999083321272},"8591735035570"]
["TECHNIK","VK 20 DL",null,"Vystřihovací kleště na plastové kanály, šíře čelistí 20mm, dlouhé rukojeti","1ks",46.019498907036898,{"$f":"F5913*(1-Elteq!$F$9)","v":46.019498907036898},"8591735051358"]
["TECHNIK","VK 24",null,"Vystřihovací kleště na plastové kabelové kanály 24mm","1ks",115.04874726759225,{"$f":"F5914*(1-Elteq!$F$9)","v":115.04874726759225},"8591735040567"]
["TECHNIK","VK 26",null,"Vystřihovací kleště na plastové kanály, šíře čelistí 26mm","1ks",39.710374056878614,{"$f":"F5915*(1-Elteq!$F$9)","v":39.710374056878614},"8591735035587"]
["TECHNIK","VK 26 DL",null,"Vystřihovací kleště na plastové kanály, šíře čelistí 26mm, dlouhé rukojeti","1ks",47.132873880594246,{"$f":"F5916*(1-Elteq!$F$9)","v":47.132873880594246},"8591735051365"]
["TECHNIK","WT 1",null,"Nůžky na plastové lišty a kabelové kanály do celkové šíře 65mm","1ks",55.29762368668144,{"$f":"F5917*(1-Elteq!$F$9)","v":55.29762368668144},"8591735025267"]
["TECHNIK","WT 110",null,"950221 KNIPEX nůžky na plasty a kabelové kanály do šíře 110mm bez podpěry","1ks",88.327747902215989,{"$f":"F5918*(1-Elteq!$F$9)","v":88.327747902215989},"8591735028268"]
["TECHNIK","WT 110 P",null,"950221 KNIPEX nůžky na plasty a kabelové kanály do šíře 110mm s podpěrou","1ks",96.492497708303176,{"$f":"F5919*(1-Elteq!$F$9)","v":96.492497708303176},"8591735045999"]
["TECHNIK","WT 60",null,"950210 KNIPEX nůžky na plastové lišty a kabelové kanály do celkové šíře 60mm bez podpěry","1ks",84.98762298154395,{"$f":"F5920*(1-Elteq!$F$9)","v":84.98762298154395},"8591735028275"]
["TECHNIK","WT 85",null,"Nůžky na plastové lišty a kabelové kanály do celkové šíře 85mm","1ks",63.165473499820003,{"$f":"F5921*(1-Elteq!$F$9)","v":63.165473499820003},"8591735055097"]
["TECHNIK","UK-2 AAA akce",null,"Vodotěsná xenonová svítilna 1W","1ks",12.172899710893631,{"$f":"F5922*(1-Elteq!$F$9)","v":12.172899710893631},""]
["TECHNIK","UK-4 AA",null,"Vodotěsná xenonová svítilna 2W","1ks",35.071311667056349,{"$f":"F5923*(1-Elteq!$F$9)","v":35.071311667056349},""]
["TECHNIK","KN 98 20 10",null,"982010 KNIPEX šroubovák plochý do 1000V Kraftform 1,6x10x200mm","1ks",16.737737102478743,{"$f":"F5924*(1-Elteq!$F$9)","v":16.737737102478743},"8591735055226"]
["TECHNIK","KN 98 20 25",null,"982025 KNIPEX šroubovák plochý do 1000V Kraftform 0,4x2,5x75mm","1ks",5.6039873669053,{"$f":"F5925*(1-Elteq!$F$9)","v":5.6039873669053},"8591735055233"]
["TECHNIK","KN 98 20 30",null,"982030 KNIPEX šroubovák plochý do 1000V Kraftform 0,5x3,0x100mm","1ks",6.1235623545653937,{"$f":"F5926*(1-Elteq!$F$9)","v":6.1235623545653937},"8591735042301"]
["TECHNIK","KN 98 20 35",null,"982035 KNIPEX šroubovák plochý do 1000V Kraftform 0,6x3,5x100mm","1ks",6.0122248572096595,{"$f":"F5927*(1-Elteq!$F$9)","v":6.0122248572096595},"8591735055240"]
["TECHNIK","KN 98 20 40",null,"982040 KNIPEX šroubovák plochý do 1000V Kraftform 0,8x4,0x100mm","1ks",6.5317998448697541,{"$f":"F5928*(1-Elteq!$F$9)","v":6.5317998448697541},"8591735055257"]
["TECHNIK","KN 98 20 55",null,"982055 KNIPEX šroubovák plochý do 1000V Kraftform 1,0x5,5x125mm","1ks",7.7936248149014107,{"$f":"F5929*(1-Elteq!$F$9)","v":7.7936248149014107},"8591735055264"]
["TECHNIK","KN 98 20 65",null,"982065 KNIPEX šroubovák plochý do 1000V Kraftform 1,2x6,5x150mm","1ks",9.5007997743560058,{"$f":"F5930*(1-Elteq!$F$9)","v":9.5007997743560058},"8591735055271"]
["TECHNIK","KN 98 20 80",null,"982080 KNIPEX šroubovák plochý do 1000V Kraftform 1,2x8,0x150mm","1ks",12.358462206486523,{"$f":"F5931*(1-Elteq!$F$9)","v":12.358462206486523},"8591735055288"]
["TECHNIK","KN 98 24 00",null,"982400 KNIPEX šroubovák křížový do 1000V Kraftform Phillips PH 0x60mm","1ks",6.1235623545653937,{"$f":"F5932*(1-Elteq!$F$9)","v":6.1235623545653937},"8591735055295"]
["TECHNIK","KN 98 24 01",null,"982401 KNIPEX šroubovák křížový do 1000V Kraftform Phillips PH 1x80mm","1ks",7.7565123157828326,{"$f":"F5933*(1-Elteq!$F$9)","v":7.7565123157828326},"8591735042318"]
["TECHNIK","KN 98 24 02",null,"982402 KNIPEX šroubovák křížový do 1000V Kraftform Phillips PH 2x100mm","1ks",9.1296747831702234,{"$f":"F5934*(1-Elteq!$F$9)","v":9.1296747831702234},"8591735055301"]
["TECHNIK","KN 98 24 03",null,"982403 KNIPEX šroubovák křížový do 1000V Kraftform Phillips PH 3x150mm","1ks",12.544024702079414,{"$f":"F5935*(1-Elteq!$F$9)","v":12.544024702079414},"8591735055318"]
["TECHNIK","KN 98 24 04",null,"982404 KNIPEX šroubovák křížový do 1000V Kraftform Phillips PH 4x200mm","1ks",16.477949608648697,{"$f":"F5936*(1-Elteq!$F$9)","v":16.477949608648697},"8591735055325"]
["TECHNIK","Sada Phillips",null,"Sada 6ks šroubováků 1000V Kraftform (0,4x2,5x80/0,6x3,5x100/0,8x4x100/1,0x5,5x125/PH1/PH2)","1sada",38.931011575388474,{"$f":"F5937*(1-Elteq!$F$9)","v":38.931011575388474},"8591735021719"]
["TECHNIK","Sada Pozidriv",null,"Sada 6ks šroubováků 1000V Kraftform (0,4x2,5x80/0,6x3,5x100/0,8x4x100/1,0x5,5x125/PZ1/PZ2)","1sada",40.526849037487338,{"$f":"F5938*(1-Elteq!$F$9)","v":40.526849037487338},"8591735021726"]
["TECHNIK","SR  2,5x 80",null,"Šroubovák plochý 1000V Kraftform 0,4x2,5x80mm","1ks",5.1586373774823624,{"$f":"F5939*(1-Elteq!$F$9)","v":5.1586373774823624},"8591735038175"]
["TECHNIK","SR  3,0x100",null,"Šroubovák plochý 1000V Kraftform 0,5x3,0x100mm","1ks",5.2699748748380966,{"$f":"F5940*(1-Elteq!$F$9)","v":5.2699748748380966},"8591735038182"]
["TECHNIK","SR  3,5x100",null,"Šroubovák plochý 1000V Kraftform 0,6x3,5x100mm","1ks",5.6039873669053,{"$f":"F5941*(1-Elteq!$F$9)","v":5.6039873669053},"8591735038199"]
["TECHNIK","SR  4,0x100",null,"Šroubovák plochý 1000V Kraftform 0,8x4,0x100mm","1ks",6.5689123439883321,{"$f":"F5942*(1-Elteq!$F$9)","v":6.5689123439883321},"8591735038205"]
["TECHNIK","SR  5,5 SET",null,"Sada 5ks šroubováků plochých 1000V Kraftform, rozměry 2,5-5,5mm","1sada",28.947749312490952,{"$f":"F5943*(1-Elteq!$F$9)","v":28.947749312490952},"8591735038212"]
["TECHNIK","SR  5,5x125",null,"Šroubovák plochý 1000V Kraftform 1,0x5,5x125mm","1ks",8.6100997955101306,{"$f":"F5944*(1-Elteq!$F$9)","v":8.6100997955101306},"8591735038229"]
["TECHNIK","SR  6,5 SET",null,"Sada 6ks šroubováků plochých 1000V Kraftform, rozměry 2,5-6,5mm","1sada",38.893899076269896,{"$f":"F5945*(1-Elteq!$F$9)","v":38.893899076269896},"8591735038236"]
["TECHNIK","SR  6,5x150",null,"Šroubovák plochý 1000V Kraftform 1,2x6,5x150mm","1ks",10.502837250557615,{"$f":"F5946*(1-Elteq!$F$9)","v":10.502837250557615},"8591735038243"]
["TECHNIK","SR  8,0x175",null,"Šroubovák plochý 1000V Kraftform 1,2x8,0x175mm","1ks",12.98937469150235,{"$f":"F5947*(1-Elteq!$F$9)","v":12.98937469150235},"8591735038250"]
["TECHNIK","SR 10 SET",null,"Sada 8ks šroubováků plochých 1000V Kraftform, rozměry 2,5-10mm","1sada",66.282923425780567,{"$f":"F5948*(1-Elteq!$F$9)","v":66.282923425780567},"8591735038267"]
["TECHNIK","SR 10x200",null,"Šroubovák plochý 1000V Kraftform 1,6x10,0x200mm","1ks",16.515062107767275,{"$f":"F5949*(1-Elteq!$F$9)","v":16.515062107767275},"8591735038359"]
["TECHNIK","SR PH 0",null,"Šroubovák křížový 1000V Kraftform Phillips PH 0x80mm","1ks",6.0493373563282375,{"$f":"F5950*(1-Elteq!$F$9)","v":6.0493373563282375},"8591735038274"]
["TECHNIK","SR PH 0-4 SET",null,"Sada 5ks šroubováků 1000V Kraftform, Phillips PH 0-4","1sada",49.730748818894718,{"$f":"F5951*(1-Elteq!$F$9)","v":49.730748818894718},"8591735032487"]
["TECHNIK","SR PH 1",null,"Šroubovák křížový 1000V Kraftform Phillips PH 1x80mm","1ks",7.0513748325298478,{"$f":"F5952*(1-Elteq!$F$9)","v":7.0513748325298478},"8591735038281"]
["TECHNIK","SR PH 1-3 SET",null,"Sada 3ks šroubováků 1000V Kraftform, Phillips PH 1-3","1sada",27.945711836289345,{"$f":"F5953*(1-Elteq!$F$9)","v":27.945711836289345},"8591735032494"]
["TECHNIK","SR PH 1-4 SET",null,"Sada 4ks šroubováků 1000V Kraftform, Phillips PH 1-4","1sada",44.238098949345151,{"$f":"F5954*(1-Elteq!$F$9)","v":44.238098949345151},"8591735038298"]
["TECHNIK","SR PH 2",null,"Šroubovák křížový 1000V Kraftform Phillips PH 2x100mm","1ks",9.9090372646603644,{"$f":"F5955*(1-Elteq!$F$9)","v":9.9090372646603644},"8591735038304"]
["TECHNIK","SR PH 3",null,"Šroubovák křížový 1000V Kraftform Phillips PH 3x150mm","1ks",13.02648719062093,{"$f":"F5956*(1-Elteq!$F$9)","v":13.02648719062093},"8591735038311"]
["TECHNIK","SR PH 4",null,"Šroubovák křížový 1000V Kraftform Phillips PH 4x200mm","1ks",17.851112076036088,{"$f":"F5957*(1-Elteq!$F$9)","v":17.851112076036088},"8591735038328"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"SR PZ 0",null,"Šroubovák křížový 1000V Kraftform Pozidriv PZ 0x80mm","1ks",7.3482748254784731,{"$f":"F5958*(1-Elteq!$F$9)","v":7.3482748254784731},"8591735038335"]
["TECHNIK","SR PZ 0-4 SET",null,"Sada 5ks šroubováků 1000V Kraftform, Pozidriv PZ 0-4","1sada",57.264586139966077,{"$f":"F5959*(1-Elteq!$F$9)","v":57.264586139966077},"8591735032500"]
["TECHNIK","SR PZ 1",null,"Šroubovák křížový 1000V Kraftform Pozidriv PZ 1x80mm","1ks",7.9049623122571449,{"$f":"F5960*(1-Elteq!$F$9)","v":7.9049623122571449},"8591735038342"]
["TECHNIK","SR PZ 1-3 SET",null,"Sada 3ks šroubováků 1000V Kraftform, Pozidriv PZ 1-3","1sada",32.621886725230191,{"$f":"F5961*(1-Elteq!$F$9)","v":32.621886725230191},"8591735032517"]
["TECHNIK","SR PZ 1-4 SET",null,"Sada 4ks šroubováků 1000V Kraftform, Pozidriv PZ 1-4","1sada",50.398773803029123,{"$f":"F5962*(1-Elteq!$F$9)","v":50.398773803029123},"8591735038397"]
["TECHNIK","SR PZ 2",null,"Šroubovák křížový 1000V Kraftform Pozidriv PZ 2x100mm","1ks",11.579099724996382,{"$f":"F5963*(1-Elteq!$F$9)","v":11.579099724996382},"8591735038380"]
["TECHNIK","SR PZ 3",null,"Šroubovák křížový 1000V Kraftform Pozidriv PZ 3x150mm","1ks",14.80788714831268,{"$f":"F5964*(1-Elteq!$F$9)","v":14.80788714831268},"8591735038373"]
["TECHNIK","SR PZ 4",null,"Šroubovák křížový 1000V Kraftform Pozidriv PZ 4x200mm","1ks",19.187162044304902,{"$f":"F5965*(1-Elteq!$F$9)","v":19.187162044304902},"8591735038366"]
["TECHNIK","SR TX10",null,"Šroubovák Torx Kraftform TX10, délka čepele 80mm / celkem 161mm","1ks",6.0493373563282375,{"$f":"F5966*(1-Elteq!$F$9)","v":6.0493373563282375},"8591735041007"]
["TECHNIK","SR TX15",null,"Šroubovák Torx Kraftform TX15, délka čepele 80mm / celkem 178mm","1ks",6.2720123510397068,{"$f":"F5967*(1-Elteq!$F$9)","v":6.2720123510397068},"8591735041014"]
["TECHNIK","SR TX25",null,"Šroubovák Torx Kraftform TX25, délka čepele 100mm / celkem 205mm","1ks",7.19982482900416,{"$f":"F5968*(1-Elteq!$F$9)","v":7.19982482900416},"8591735041021"]
["TECHNIK","SR TX27",null,"Šroubovák Torx Kraftform TX27, délka čepele 115mm / celkem 220mm","1ks",7.9049623122571449,{"$f":"F5969*(1-Elteq!$F$9)","v":7.9049623122571449},"8591735041038"]
["TECHNIK","SR TX30",null,"Šroubovák Torx Kraftform TX30, délka čepele 115mm / celkem 220mm","1ks",8.2389748043243483,{"$f":"F5970*(1-Elteq!$F$9)","v":8.2389748043243483},"8591735041045"]
["TECHNIK","TO 4040052",null,"Zásobníkový šroubovák s ráčnou a bity, polohovatelný vč. pouzdra, 23-dílná sada","1ks",27.83437433893361,{"$f":"F5971*(1-Elteq!$F$9)","v":27.83437433893361},"8591735049829"]
["TECHNIK","TO 4060045",null,"T-šroubovák s ráčnou a teleskopický šroubovák s bity vč. pouzdra, 44-dílná sada","1ks",51.02968628804495,{"$f":"F5972*(1-Elteq!$F$9)","v":51.02968628804495},"8591735049836"]
["TECHNIK","WH 00883",null,"Šroubovák torx T10x60mm","1ks",8.8327747902215989,{"$f":"F5973*(1-Elteq!$F$9)","v":8.8327747902215989},""]
["TECHNIK","WH 00884",null,"Šroubovák torx T15x80mm","1ks",8.9812247866959112,{"$f":"F5974*(1-Elteq!$F$9)","v":8.9812247866959112},""]
["TECHNIK","WH 00885",null,"Šroubovák torx T20x80mm","1ks",9.0925622840516453,{"$f":"F5975*(1-Elteq!$F$9)","v":9.0925622840516453},""]
["TECHNIK","WH 00888",null,"Šroubovák torx T30x100mm","1ks",10.243049756727569,{"$f":"F5976*(1-Elteq!$F$9)","v":10.243049756727569},""]
["TECHNIK","WH 00889",null,"Šroubovák torx T40x150mm","1ks",11.059524737336288,{"$f":"F5977*(1-Elteq!$F$9)","v":11.059524737336288},""]
["TECHNIK","WH 03763",null,"Šroubovák torx T45x150mm","1ks",12.61824970031657,{"$f":"F5978*(1-Elteq!$F$9)","v":12.61824970031657},""]
["TECHNIK","WR 003484",null,"Sada 16 dílů šroubováků WERA Kaftform Kompakt VDE 60 iS/65 iA/67 iS/16","1sada",52.959536242211016,{"$f":"F5979*(1-Elteq!$F$9)","v":52.959536242211016},""]
["TECHNIK","WR 005315",null,"Izolovaný klíč SW 8,0 mm","1ks",24.345799421787262,{"$f":"F5980*(1-Elteq!$F$9)","v":24.345799421787262},""]
["TECHNIK","WR 005325",null,"Izolovaný klíč SW 10,0 mm","1ks",28.502399323068015,{"$f":"F5981*(1-Elteq!$F$9)","v":28.502399323068015},""]
["TECHNIK","WR 006184",null,"Šroubovák TORX izolovaný do 1000V, TX 8 x 80mm","1ks",8.053412308731458,{"$f":"F5982*(1-Elteq!$F$9)","v":8.053412308731458},""]
["TECHNIK","WR 008775",null,"Šroubovák křížový Phillips PH 01x25mm","1ks",6.2348998519211287,{"$f":"F5983*(1-Elteq!$F$9)","v":6.2348998519211287},""]
["TECHNIK","WR 008780",null,"Šroubovák křížový Phillips PH 02x25mm","1ks",6.8658123369369566,{"$f":"F5984*(1-Elteq!$F$9)","v":6.8658123369369566},""]
["TECHNIK","WR 017005",null,"Šroubovák křížový Phillips PH1, délka 80mm s úderovou koncovkou","1ks",7.3482748254784731,{"$f":"F5985*(1-Elteq!$F$9)","v":7.3482748254784731},""]
["TECHNIK","WR 017010",null,"Šroubovák křížový Phillips PH2, délka 100mm s úderovou koncovkou","1ks",10.317274754964725,{"$f":"F5986*(1-Elteq!$F$9)","v":10.317274754964725},""]
["TECHNIK","WR 017015",null,"Šroubovák křížový Phillips PH3, délka 150mm s úderovou koncovkou","1ks",15.104787141261305,{"$f":"F5987*(1-Elteq!$F$9)","v":15.104787141261305},""]
["TECHNIK","WR 018260",null,"Šroubovák plochý 0,6x3,5x80mm s úderovou koncovkou","1ks",5.6782123651424561,{"$f":"F5988*(1-Elteq!$F$9)","v":5.6782123651424561},""]
["TECHNIK","WR 018262",null,"Šroubovák plochý 0,8x4,5x90mm s úderovou koncovkou","1ks",6.2720123510397068,{"$f":"F5989*(1-Elteq!$F$9)","v":6.2720123510397068},""]
["TECHNIK","WR 018264",null,"Šroubovák plochý 1,0x5,5x100mm s úderovou koncovkou","1ks",8.4616497990358166,{"$f":"F5990*(1-Elteq!$F$9)","v":8.4616497990358166},""]
["TECHNIK","WR 018266",null,"Šroubovák plochý 1,2x7,0x125mm s úderovou koncovkou","1ks",10.317274754964725,{"$f":"F5991*(1-Elteq!$F$9)","v":10.317274754964725},""]
["TECHNIK","WR 018268",null,"Šroubovák plochý 1,6x9,0x150mm s úderovou koncovkou","1ks",13.694512174755335,{"$f":"F5992*(1-Elteq!$F$9)","v":13.694512174755335},""]
["TECHNIK","WR 018282",null,"Sada sekacích šroubováků, 4xpřímý, 2xPhillips","1sada",49.174061332116047,{"$f":"F5993*(1-Elteq!$F$9)","v":49.174061332116047},"8591735021733"]
["TECHNIK","WR 018287",null,"Sada sekacích šroubováků, 4xpřímý, 2xPozidriv","1sada",49.174061332116047,{"$f":"F5994*(1-Elteq!$F$9)","v":49.174061332116047},"8591735021740"]
["TECHNIK","WR 022086",null,"Sada 9ks zástrčných klíčů inbus Hex-Plus","1sada",14.62232465271979,{"$f":"F5995*(1-Elteq!$F$9)","v":14.62232465271979},"8591735049843"]
["TECHNIK","WR 022800",null,"Inbusový klíč SW 2,0x100mm","1ks",6.8286998378183785,{"$f":"F5996*(1-Elteq!$F$9)","v":6.8286998378183785},""]
["TECHNIK","WR 022805",null,"Inbusový klíč SW 3,0x100mm","1ks",7.0884873316484258,{"$f":"F5997*(1-Elteq!$F$9)","v":7.0884873316484258},""]
["TECHNIK","WR 023105",null,"Šroubovák HEX-PLUS inbus 2,0mm","1ks",5.3813123721938307,{"$f":"F5998*(1-Elteq!$F$9)","v":5.3813123721938307},""]
["TECHNIK","WR 031200",null,"Šroubovák plochý 1,2x6,5x150mm","1ks",6.9029248360555355,{"$f":"F5999*(1-Elteq!$F$9)","v":6.9029248360555355},""]
["TECHNIK","WR 031209",null,"Šroubovák plochý 0,4x2,5x75mm","1ks",3.4885749171463458,{"$f":"F6000*(1-Elteq!$F$9)","v":3.4885749171463458},""]
["TECHNIK","WR 031210",null,"Šroubovák plochý 0,5x3,0x80mm","1ks",3.7483624109763927,{"$f":"F6001*(1-Elteq!$F$9)","v":3.7483624109763927},""]
["TECHNIK","WR 031211",null,"Šroubovák plochý 0,8x4,0x100mm","1ks",4.00814990480644,{"$f":"F6002*(1-Elteq!$F$9)","v":4.00814990480644},""]
["TECHNIK","WR 031212",null,"Šroubovák plochý 1,0x5,5x125mm","1ks",6.0122248572096595,{"$f":"F6003*(1-Elteq!$F$9)","v":6.0122248572096595},""]
["TECHNIK","WR 031219",null,"Šroubovák křížový Phillips PH 0x60mm","1ks",3.9339249065692834,{"$f":"F6004*(1-Elteq!$F$9)","v":3.9339249065692834},""]
["TECHNIK","WR 031220",null,"Šroubovák křížový Phillips PH 1x80mm","1ks",4.6390623898222678,{"$f":"F6005*(1-Elteq!$F$9)","v":4.6390623898222678},""]
["TECHNIK","WR 031221",null,"Šroubovák křížový Phillips PH 2x100mm","1ks",6.2348998519211287,{"$f":"F6006*(1-Elteq!$F$9)","v":6.2348998519211287},""]
["TECHNIK","WR 031225",null,"Šroubovák křížový Pozidriv PZ 1x80mm","1ks",5.3441998730752527,{"$f":"F6007*(1-Elteq!$F$9)","v":5.3441998730752527},""]
["TECHNIK","WR 031226",null,"Šroubovák křížový Pozidriv PZ 2x100mm","1ks",7.4596123228342073,{"$f":"F6008*(1-Elteq!$F$9)","v":7.4596123228342073},""]
["TECHNIK","WR 031401",null,"Šroubovák plochý 0,4x2,5x75mm","1ks",4.2679373986364864,{"$f":"F6009*(1-Elteq!$F$9)","v":4.2679373986364864},""]
["TECHNIK","WR 031402",null,"Šroubovák plochý 0,5x3x80mm","1ks",4.6761748889408468,{"$f":"F6010*(1-Elteq!$F$9)","v":4.6761748889408468},""]
["TECHNIK","WR 031408",null,"Šroubovák plochý 0,8x4x100mm","1ks",5.641099866023878,{"$f":"F6011*(1-Elteq!$F$9)","v":5.641099866023878},"8591735021757"]
["TECHNIK","WR 031412",null,"Šroubovák plochý 1,0x5,5x125mm","1ks",8.4987622981543947,{"$f":"F6012*(1-Elteq!$F$9)","v":8.4987622981543947},""]
["TECHNIK","WR 031415",null,"Šroubovák plochý 1,0x5,5x300mm","1ks",10.577062248794771,{"$f":"F6013*(1-Elteq!$F$9)","v":10.577062248794771},""]
["TECHNIK","WR 031427",null,"Šroubovák plochý 1,6x10x200mm","1ks",15.99548712010718,{"$f":"F6014*(1-Elteq!$F$9)","v":15.99548712010718},"8591735021764"]
["TECHNIK","WR 031440",null,"Šroubovák křížový Phillips PH 0x60mm","1ks",5.5668748677867219,{"$f":"F6015*(1-Elteq!$F$9)","v":5.5668748677867219},"8591735021771"]
["TECHNIK","WR 031441",null,"Šroubovák křížový Phillips PH 1x80mm","1ks",6.5689123439883321,{"$f":"F6016*(1-Elteq!$F$9)","v":6.5689123439883321},""]
["TECHNIK","WR 031442",null,"Šroubovák křížový Phillips PH 1x200mm","1ks",8.3874248007986605,{"$f":"F6017*(1-Elteq!$F$9)","v":8.3874248007986605},""]
["TECHNIK","WR 031444",null,"Šroubovák křížový Phillips PH 2x100mm","1ks",8.869887289340177,{"$f":"F6018*(1-Elteq!$F$9)","v":8.869887289340177},""]
["TECHNIK","WR 031445",null,"Šroubovák křížový Phillips PH 2x200mm","1ks",10.577062248794771,{"$f":"F6019*(1-Elteq!$F$9)","v":10.577062248794771},""]
["TECHNIK","WR 031451",null,"Šroubovák křížový Phillips PH 1x80mm","1ks",7.8307373140199887,{"$f":"F6020*(1-Elteq!$F$9)","v":7.8307373140199887},"8591735021788"]
["TECHNIK","WR 031461",null,"Šroubovák křížový Pozidriv PZ 1x80mm","1ks",7.6080623193085195,{"$f":"F6021*(1-Elteq!$F$9)","v":7.6080623193085195},"8591735021795"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"WR 031501",null,"Šroubovák torx TX 6","1ks",5.8266623616167692,{"$f":"F6022*(1-Elteq!$F$9)","v":5.8266623616167692},""]
["TECHNIK","WR 031502",null,"Šroubovák torx TX 7","1ks",5.7895498624981911,{"$f":"F6023*(1-Elteq!$F$9)","v":5.7895498624981911},""]
["TECHNIK","WR 031503",null,"Šroubovák torx TX 8","1ks",5.7895498624981911,{"$f":"F6024*(1-Elteq!$F$9)","v":5.7895498624981911},""]
["TECHNIK","WR 031504",null,"Šroubovák torx TX 9","1ks",6.1977873528025507,{"$f":"F6025*(1-Elteq!$F$9)","v":6.1977873528025507},""]
["TECHNIK","WR 031505",null,"Šroubovák torx TX 10","1ks",6.3462373492768629,{"$f":"F6026*(1-Elteq!$F$9)","v":6.3462373492768629},""]
["TECHNIK","WR 031506",null,"Šroubovák torx TX 15","1ks",6.4575748466325971,{"$f":"F6027*(1-Elteq!$F$9)","v":6.4575748466325971},""]
["TECHNIK","WR 031575",null,"Sada šroubováků WERA do 1000V, 4xpřímý, 2xPhillips","1sada",34.848636672344881,{"$f":"F6028*(1-Elteq!$F$9)","v":34.848636672344881},"8591735021801"]
["TECHNIK","WR 031576",null,"Sada šroubováků WERA do 1000V, 4xpřímý, 2xPozidriv","1sada",34.848636672344881,{"$f":"F6029*(1-Elteq!$F$9)","v":34.848636672344881},"8591735021818"]
["TECHNIK","WR 051019",null,"Profesionální zásobníkový šroubovák Kraftform WERA","1ks",48.172023855914432,{"$f":"F6030*(1-Elteq!$F$9)","v":48.172023855914432},""]
["TECHNIK","WR 073593",null,"Sada 9ks zástrčných klíčů inbus Hex-Plus, barevná profi WERA","1sada",27.240574353036358,{"$f":"F6031*(1-Elteq!$F$9)","v":27.240574353036358},"8591735049515"]
["TECHNIK","WR 110069",null,"Šroubovák plochý 0,8x4,0x25","1ks",6.1235623545653937,{"$f":"F6032*(1-Elteq!$F$9)","v":6.1235623545653937},""]
["TECHNIK","WR 118150",null,"Sada micro šroubováků WERA, 4xpřímý, 2xPhillips (1,8x60/2,0x60/2,5x60/3,0x80/PH00x60/PH0x60)","1sada",30.024011786929719,{"$f":"F6033*(1-Elteq!$F$9)","v":30.024011786929719},"8591735021825"]
["TECHNIK","WR 118152",null,"Sada micro šroubováků WERA, 4xpřímý, 2xPhillips (2,5x80/3,0x80/3,5x80/4,0x80/PH0x60/PH1x80)","1sada",30.024011786929719,{"$f":"F6034*(1-Elteq!$F$9)","v":30.024011786929719},"8591735021832"]
["TECHNIK","WR 138070",null,"Šroubovák WERA se šestihrannou kulovou hlavou rozměr 2,5x100mm","1ks",7.0884873316484258,{"$f":"F6035*(1-Elteq!$F$9)","v":7.0884873316484258},""]
["TECHNIK","AT-44",null,"Technický sprej - všestranný, velmi účinný prostředek s teflonem pro nižší tření (400 ml)","1ks",13.100712188858086,{"$f":"F6036*(1-Elteq!$F$9)","v":13.100712188858086},""]
["TECHNIK","Bio - Cut",null,"Technický sprej - kvalitní řezací olej pro vrtání, soustružení, frézování a řezání (400 ml)","1ks",15.216124638617039,{"$f":"F6037*(1-Elteq!$F$9)","v":15.216124638617039},""]
["TECHNIK","Bio - Fluid",null,"Technický sprej - vysoce čistý minerální olej pro potravinářský a farmaceutický průmysl (500 ml)","1ks",15.80992462451429,{"$f":"F6038*(1-Elteq!$F$9)","v":15.80992462451429},""]
["TECHNIK","BLACK SEAL SILIKON",null,"Speciální WEICON black seal silikon bez rozpouštědel, teplotní odolnost od -60°C až +280°C (310 ml)","1ks",13.360499682688133,{"$f":"F6039*(1-Elteq!$F$9)","v":13.360499682688133},""]
["TECHNIK","CLEAR GLIDE",null,"Lubrikant na protahování kabelů (0,95 litru)","1ks",14.473874656245476,{"$f":"F6040*(1-Elteq!$F$9)","v":14.473874656245476},""]
["TECHNIK","Cockpit sprej",null,"Technický sprej - univerzální prostředek na ošetření umělých hmot a gumy, odpuzuje vodu (400 ml)","1ks",7.4967248219527853,{"$f":"F6041*(1-Elteq!$F$9)","v":7.4967248219527853},""]
["TECHNIK","Corro ochrana sprej",null,"Technický sprej - dočasná protikorozní ochrana pro vnitřní uložení kovů (400 ml)","1ks",9.9832622628975205,{"$f":"F6042*(1-Elteq!$F$9)","v":9.9832622628975205},""]
["TECHNIK","Čistič brzd",null,"Technický sprej - univerzální čistič pro automobilovou oblast, nezanechává žádné stopy (500 ml)","1ks",7.274049827241317,{"$f":"F6043*(1-Elteq!$F$9)","v":7.274049827241317},""]
["TECHNIK","Čistič el. kontaktů",null,"Technický sprej - univerzální čistič a odmašťovač elektrotechnických součástí (400 ml)","1ks",11.653324723233538,{"$f":"F6044*(1-Elteq!$F$9)","v":11.653324723233538},"8591735049805"]
["TECHNIK","Čistič hořáků",null,"Technický sprej - pro odmaštění hořáků při zašpinění tuky, oleji, sazemi a pod. nečistotami (500 ml)","1ks",8.3131998025615044,{"$f":"F6045*(1-Elteq!$F$9)","v":8.3131998025615044},""]
["TECHNIK","Čistič plastů sprej",null,"Technický sprej - prostředek k čištění a odmaštění citlivých plastových povrchů (500 ml)","1ks",9.4636872752374277,{"$f":"F6046*(1-Elteq!$F$9)","v":9.4636872752374277},""]
["TECHNIK","Čistič S sprej",null,"Technický sprej - odmašťuje a čistí všechny kovy, sklo, keramiku a plastické hmoty (500 ml)","1ks",8.4245372999172385,{"$f":"F6047*(1-Elteq!$F$9)","v":8.4245372999172385},""]
["TECHNIK","Hledač netěsností",null,"Technický sprej - spolehlivě vyhledává netěsnosti a praskliny v potrubích a zařízeních (400 ml)","1ks",8.3131998025615044,{"$f":"F6048*(1-Elteq!$F$9)","v":8.3131998025615044},""]
["TECHNIK","Hliníkový sprej",null,"Technický sprej - protikorozní ochrana s vysokou tepelnou odolností, obsahuje 99,5% hliníku (400 ml)","1ks",13.731624673873913,{"$f":"F6049*(1-Elteq!$F$9)","v":13.731624673873913},""]
["TECHNIK","Chladící sprej",null,"Technický sprej - k vyhledávání chyb v elektrotechnice a k opravářskýn účelům v průmyslu (400 ml)","1ks",14.362537158889742,{"$f":"F6050*(1-Elteq!$F$9)","v":14.362537158889742},""]
["TECHNIK","Chrom sprej",null,"Technický sprej - vysoce lesklý a odolný proti povětrnostním vlivům, chrání proti korozi (400 ml)","1ks",14.770774649194102,{"$f":"F6051*(1-Elteq!$F$9)","v":14.770774649194102},""]
["TECHNIK","Lepidlo ve spreji",null,"Technický sprej - čisté, rychlé a jednoduché lepidlo ke spojování lehkých materiálů (500 ml)","1ks",12.061562213537897,{"$f":"F6052*(1-Elteq!$F$9)","v":12.061562213537897},""]
["TECHNIK","Měď sprej",null,"Technický sprej - kov odolný povětrnostním vlivům k ochraně a úpravě různých materiálů (400 ml)","1ks",15.624362128921399,{"$f":"F6053*(1-Elteq!$F$9)","v":15.624362128921399},""]
["TECHNIK","Metal Fluid sprej",null,"Technický sprej - produkt na bázi vosku pro čištění a ochranu především kovových povrchů (400 ml)","1ks",16.255274613937228,{"$f":"F6054*(1-Elteq!$F$9)","v":16.255274613937228},""]
["TECHNIK","Mosaz sprej",null,"Technický sprej - kov k ochraně a optické úpravě různých materiálů (400 ml)","1ks",15.624362128921399,{"$f":"F6055*(1-Elteq!$F$9)","v":15.624362128921399},""]
["TECHNIK","Multipěnový sprej",null,"Technický sprej - universální aktivní čistící prostředek na sklo, chrom a plasty (400 ml)","1ks",7.3853873245970512,{"$f":"F6056*(1-Elteq!$F$9)","v":7.3853873245970512},""]
["TECHNIK","NOALOX",null,"Anti-oxidant pro elektrické aplikace s hliníkem (2,28 dl)","1ks",33.661036700550376,{"$f":"F6057*(1-Elteq!$F$9)","v":33.661036700550376},""]
["TECHNIK","Oddělovač forem",null,"Technický sprej - bezsilikonový kluzný a oddělovací prostředek  (400 ml)","1ks",7.7193998166642546,{"$f":"F6058*(1-Elteq!$F$9)","v":7.7193998166642546},""]
["TECHNIK","Odstraňovač etiket",null,"Technický sprej - rychle a bez námahy odstraňuje papírové etikety se zbytky lepidel (500 ml)","1ks",11.02241223821771,{"$f":"F6059*(1-Elteq!$F$9)","v":11.02241223821771},""]
["TECHNIK","Odstraňovač sprej",null,"Technický sprej - rychle a bez námahy odstraňuje zbytky těsnění a zatvrdnutých lepidel (400 ml)","1ks",11.02241223821771,{"$f":"F6060*(1-Elteq!$F$9)","v":11.02241223821771},""]
["TECHNIK","Ochr. při svařování",null,"Technický sprej - k čištění a údržbě svařovací trysky a k ochraně před ulpěním kapiček kovu (400 ml)","1ks",6.4575748466325971,{"$f":"F6061*(1-Elteq!$F$9)","v":6.4575748466325971},""]
["TECHNIK","Ochrana nerezu",null,"Technický sprej - antistatický prostředek pro čištění a ochranu povrchů z nerezu (400 ml)","1ks",14.139862164178274,{"$f":"F6062*(1-Elteq!$F$9)","v":14.139862164178274},""]
["TECHNIK","Pěna k ochraně rukou",null,"Technický sprej - nemastný ochranný film zamezující nečistotě vniknout do pórů kůže (200 ml)","1ks",16.440837109530118,{"$f":"F6063*(1-Elteq!$F$9)","v":16.440837109530118},""]
["TECHNIK","Silikonový sprej",null,"Technický sprej - čistý silikon, ideální kluzný a oddělovací prostředek pro údržbu a výrobu (400 ml)","1ks",10.836849742624819,{"$f":"F6064*(1-Elteq!$F$9)","v":10.836849742624819},""]
["TECHNIK","Sprej na řetězy,lana",null,"Technický sprej - syntetický, transperentní mazací prostředek pro namáhané části (400 ml)","1ks",11.39353722940349,{"$f":"F6065*(1-Elteq!$F$9)","v":11.39353722940349},""]
["TECHNIK","Šok na rez",null,"Technický sprej - působí studeným šokem a následně uvolní pevné spojení mezi rezavými díly (400 ml)","1ks",13.174937187095242,{"$f":"F6066*(1-Elteq!$F$9)","v":13.174937187095242},""]
["TECHNIK","Teflonový sprej",null,"Technický sprej - suchý, čistý, beztukový, dobře přilnavý a odolný mazací prostředek (400 ml)","1ks",16.255274613937228,{"$f":"F6067*(1-Elteq!$F$9)","v":16.255274613937228},""]
["TECHNIK","Tlakový vzduch",null,"Technický sprej - k odstranění prachu na nepřístupných místech a choulostivých plochách (400 ml)","1ks",13.954299668585383,{"$f":"F6068*(1-Elteq!$F$9)","v":13.954299668585383},""]
["TECHNIK","Top - Lub",null,"Technický sprej - pevně lpějící mazací prostředek pro nasazení v nejtěžších podmínkách (400 ml)","1ks",12.284237208249367,{"$f":"F6069*(1-Elteq!$F$9)","v":12.284237208249367},""]
["TECHNIK","Tuk ve spreji",null,"Technický sprej - víceúčelový tuk s dlouhou trvanlivostí na ozubená kola, kladky a ložiska (400 ml)","1ks",10.688399746150505,{"$f":"F6070*(1-Elteq!$F$9)","v":10.688399746150505},""]
["TECHNIK","Ušlechtilá ocel",null,"Technický sprej - protikorozní ochrana na základě pigmentů nerezavějících ocelí a epoxidů (400 ml)","1ks",16.440837109530118,{"$f":"F6071*(1-Elteq!$F$9)","v":16.440837109530118},""]
["TECHNIK","Uvolňovací sprej",null,"Technický sprej - uvolňuje rezavé spoje, odstraňuje vodu, zajišťuje kontakt a maže (400 ml)","1ks",6.4575748466325971,{"$f":"F6072*(1-Elteq!$F$9)","v":6.4575748466325971},""]
["TECHNIK","Uvolňovač šroubů",null,"Technický sprej - rychle uvolňuje velmi rezavé spoje, odstraňuje vodu a maže (400 ml) WERA","1ks",9.5379122734745838,{"$f":"F6073*(1-Elteq!$F$9)","v":9.5379122734745838},""]
["TECHNIK","W44T Turbo",null,"Technický sprej - uvolňuje spoje, vytlačuje vlhkost, odstraňuje skřípání, čistí, konzervuje (400 ml)","1ks",7.236937328122738,{"$f":"F6074*(1-Elteq!$F$9)","v":7.236937328122738},""]
["TECHNIK","ZH-PUR 100",null,"Zalévací hmota Scotchcast 40 pro spojky do 1kV, dvousložková na bázi polyuretanu, 100g / 90ml","1ks",7.6080623193085195,{"$f":"F6075*(1-Elteq!$F$9)","v":7.6080623193085195},"8591735037598"]
["TECHNIK","ZH-PUR 230",null,"Zalévací hmota Scotchcast 40 pro spojky do 1kV, dvousložková na bázi polyuretanu, 215g / 200ml","1ks",9.2781247796445356,{"$f":"F6076*(1-Elteq!$F$9)","v":9.2781247796445356},"8591735037581"]
["TECHNIK","ZH-PUR 426",null,"Zalévací hmota Scotchcast 40 pro spojky do 1kV, dvousložková na bázi polyuretanu, 426g / 370ml","1ks",13.731624673873913,{"$f":"F6077*(1-Elteq!$F$9)","v":13.731624673873913},""]
["TECHNIK","Zinkohliníkový sprej",null,"Technický sprej - chrání trvale všechny kovové povrchy proti korozi a chemikáliím (400 ml)","1ks",12.915149693265194,{"$f":"F6078*(1-Elteq!$F$9)","v":12.915149693265194},""]
["TECHNIK","Zinkový sprej",null,"Technický sprej - rychleschnoucí protikorozní ochrana s dlouhou životností pro všechny kovy (400 ml)","1ks",14.585212153601212,{"$f":"F6079*(1-Elteq!$F$9)","v":14.585212153601212},""]
["TECHNIK","ALFRA 1101124",null,"1101124 ALFRA kuželový záhlubník HSS pro otvory 2,8-12,4mm s cylindrickou stopkou 8mm","1ks",18.370687063696181,{"$f":"F6080*(1-Elteq!$F$9)","v":18.370687063696181},""]
["TECHNIK","PASTA",null,"Speciální pasta pro vrtání","1ks",4.824624885415159,{"$f":"F6081*(1-Elteq!$F$9)","v":4.824624885415159},""]
["TECHNIK","VK  3-14",null,"Vrták kónusový pro plech 0,1-2mm, průměr 3-14mm","1ks",13.731624673873913,{"$f":"F6082*(1-Elteq!$F$9)","v":13.731624673873913},""]
["TECHNIK","VK  4-30",null,"Vrták kónusový pro plech 0,1-2mm, průměr 4-30mm","1ks",39.673261557760036,{"$f":"F6083*(1-Elteq!$F$9)","v":39.673261557760036},""]
["TECHNIK","VK  8-20",null,"Vrták kónusový pro plech 0,1-2mm, průměr 8-20mm","1ks",18.482024561051915,{"$f":"F6084*(1-Elteq!$F$9)","v":18.482024561051915},""]
["TECHNIK","VK 16-30",null,"Vrták kónusový pro plech 0,1-2mm, průměr 16-30mm","1ks",32.176536735807254,{"$f":"F6085*(1-Elteq!$F$9)","v":32.176536735807254},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"VK 26-40",null,"Vrták kónusový pro plech 0,1-2mm, průměr 26-40mm","1ks",71.367335805025775,{"$f":"F6086*(1-Elteq!$F$9)","v":71.367335805025775},""]
["TECHNIK","VK 36-50",null,"Vrták kónusový pro plech 0,1-2mm, průměr 36-50mm","1ks",109.48187239980552,{"$f":"F6087*(1-Elteq!$F$9)","v":109.48187239980552},""]
["TECHNIK","VK 46-60",null,"Vrták kónusový pro plech 0,1-2mm, průměr 46-60mm","1ks",177.69464577975216,{"$f":"F6088*(1-Elteq!$F$9)","v":177.69464577975216},""]
["TECHNIK","VS  4-12",null,"08070 ALFRA vrták stupňovitý pro plech max. 4mm, pro otvory 4-12mm","1ks",24.865374409447359,{"$f":"F6089*(1-Elteq!$F$9)","v":24.865374409447359},""]
["TECHNIK","VS  6-20",null,"08071 ALFRA vrták stupňovitý pro plech max. 4mm, pro otvory 6-20mm","1ks",32.844561719941659,{"$f":"F6090*(1-Elteq!$F$9)","v":32.844561719941659},""]
["TECHNIK","VS  6-30",null,"08072 ALFRA vrták stupňovitý pro plech max. 4mm, pro otvory 6-30mm","1ks",55.483186182274331,{"$f":"F6091*(1-Elteq!$F$9)","v":55.483186182274331},""]
["TECHNIK","VS 30-40",null,"Vrták stupňovitý pro plech max. 4mm, pro otvory 30-40mm","1ks",121.32075961863195,{"$f":"F6092*(1-Elteq!$F$9)","v":121.32075961863195},""]
["TECHNIK","VS 40-50",null,"Vrták stupňovitý pro plech max. 4mm, pro otvory 40-50mm","1ks",199.36834526500181,{"$f":"F6093*(1-Elteq!$F$9)","v":199.36834526500181},""]
["TECHNIK","VS 50-60",null,"Vrták stupňovitý pro plech max. 4mm, pro otvory 50-60mm","1ks",294.04233051649464,{"$f":"F6094*(1-Elteq!$F$9)","v":294.04233051649464},""]
["TECHNIK","VS AM",null,"08001 ALFRA vrták stupňovitý pro plech max. 4mm, pro otvory 9-36mm","1ks",136.20287176518178,{"$f":"F6095*(1-Elteq!$F$9)","v":136.20287176518178},""]
["TECHNIK","VS AM-1",null,"08002 ALFRA vrták stupňovitý pro plech max. 4mm, pro otvory 25-58mm","1ks",225.08730715417644,{"$f":"F6096*(1-Elteq!$F$9)","v":225.08730715417644},""]
["TECHNIK","VS AM-TIN",null,"08037 ALFRA vrták stupňovitý pro plech max. 4mm, pro otvory 9-36mm TIN","1ks",175.17099583968886,{"$f":"F6097*(1-Elteq!$F$9)","v":175.17099583968886},""]
["TECHNIK","VS MF",null,"Vrták stupňovitý pro plech max.4mm, pro otvory 10,5-40,5mm","1ks",120.24449714419319,{"$f":"F6098*(1-Elteq!$F$9)","v":120.24449714419319},"8591735054663"]
["TECHNIK","VS PG",null,"Vrták stupňovitý pro plech max. 4mm, pro otvory 11,4-30,5mm","1ks",96.121372717117396,{"$f":"F6099*(1-Elteq!$F$9)","v":96.121372717117396},"8591735018870"]
["TECHNIK","VS PVD",null,"08003 ALFRA vrták stupňovitý pro plech max. 4mm, pro otvory 12,5-40,0mm","1ks",102.43049756727568,{"$f":"F6100*(1-Elteq!$F$9)","v":102.43049756727568},""]
["TECHNIK","VS PVD-TIN",null,"08004 ALFRA vrták stupňovitý pro plech max. 4mm, pro otvory 12,5-40,0mm TIN","1ks",200.40749524032199,{"$f":"F6101*(1-Elteq!$F$9)","v":200.40749524032199},""]
["TECHNIK","VS PVK",null,"08005 ALFRA vrták stupňovitý pro plech max. 4mm, pro otvory 12,5-28,3mm","1ks",99.461497637789435,{"$f":"F6102*(1-Elteq!$F$9)","v":99.461497637789435},""]
["TECHNIK","VS SET 4-30",null,"08073 ALFRA sada stupňovitých vrtáků 4-12, 6-20 a 6-30mm (dříve 08012)","1sada",144.36762157126898,{"$f":"F6103*(1-Elteq!$F$9)","v":144.36762157126898},""]
["TECHNIK","VRE 0104",null,"Vypichovač kontaktů Coninvers RC-59S2, RC-5AS2, RC-5CS2","1ks",32.287874233162988,{"$f":"F6104*(1-Elteq!$F$9)","v":32.287874233162988},""]
["TECHNIK","VRE 0204",null,"Vypichovač kontaktů Coninvers RC-6RS2, RC-62S2, RC-6KS2, RC-67S2","1ks",32.287874233162988,{"$f":"F6105*(1-Elteq!$F$9)","v":32.287874233162988},""]
["TECHNIK","VRE 0304",null,"Vypichovač kontaktů Coninvers SC-79P2, SC-72P2, SC-7AP2, SC-7VP2","1ks",32.287874233162988,{"$f":"F6106*(1-Elteq!$F$9)","v":32.287874233162988},""]
["TECHNIK","VRE 0404",null,"Vypichovač kontaktů Coninvers RC-58S2000, RC-58P2000","1ks",35.62799915383502,{"$f":"F6107*(1-Elteq!$F$9)","v":35.62799915383502},""]
["TECHNIK","VRE 0504",null,"Vypichovač kontaktů ILME-CDF/CDM, HTS-HDN, Harting-0915000, Contact-HDØ1,6mm, Phöenix-HC-D, Wieland","1ks",41.937124003993304,{"$f":"F6108*(1-Elteq!$F$9)","v":41.937124003993304},"8591735035594"]
["TECHNIK","VRE 0524",null,"Vypichovač kontaktů CDM-RM kontaktsystém","1ks",41.937124003993304,{"$f":"F6109*(1-Elteq!$F$9)","v":41.937124003993304},""]
["TECHNIK","VRE 0534",null,"Vypichovač kontaktů ILME-CDDF 42, CDDM 42, CDF 15, CDM 15","1ks",32.287874233162988,{"$f":"F6110*(1-Elteq!$F$9)","v":32.287874233162988},""]
["TECHNIK","VRE 0554",null,"Vypichovač kontaktů HTS-HDM kontakty","1ks",41.937124003993304,{"$f":"F6111*(1-Elteq!$F$9)","v":41.937124003993304},""]
["TECHNIK","VRE 0604",null,"Vypichovač kontaktů HTS-HVTO2,4mm, Contact-MCO2,5mm, Wieland-pinO2,5mm","1ks",41.937124003993304,{"$f":"F6112*(1-Elteq!$F$9)","v":41.937124003993304},""]
["TECHNIK","VRE 0704",null,"Vypichovač kontaktů HTS-HSM, Contact-MCO3,6mm, Wieland-pinO3,6mm","1ks",41.937124003993304,{"$f":"F6113*(1-Elteq!$F$9)","v":41.937124003993304},""]
["TECHNIK","VRE 0714",null,"Vypichovač kontaktů HTS-HAN","1ks",41.937124003993304,{"$f":"F6114*(1-Elteq!$F$9)","v":41.937124003993304},""]
["TECHNIK","VRE 0754",null,"Vypichovač kontaktů HTS-HSK kontakty","1ks",41.937124003993304,{"$f":"F6115*(1-Elteq!$F$9)","v":41.937124003993304},""]
["TECHNIK","VRE 0804",null,"Vypichovač kontaktů HTS-HSS kontakty","1ks",41.937124003993304,{"$f":"F6116*(1-Elteq!$F$9)","v":41.937124003993304},""]
["TECHNIK","VRE 0904",null,"Vypichovač kontaktů ILME-CXFA/CXMAO3,6mm bez pera, Harting-0932000","1ks",35.62799915383502,{"$f":"F6117*(1-Elteq!$F$9)","v":35.62799915383502},""]
["TECHNIK","VRE 1004",null,"Vypichovač kontaktů ILME-CDFA/CDFD/CDMA/CDMD, HTS-HMD, Harting-0915000, Contact-HDO1,6mm, HC-D","1ks",35.62799915383502,{"$f":"F6118*(1-Elteq!$F$9)","v":35.62799915383502},""]
["TECHNIK","VRE 1014",null,"Vypichovač kontaktů Neutrik-D-Sub","1ks",35.62799915383502,{"$f":"F6119*(1-Elteq!$F$9)","v":35.62799915383502},""]
["TECHNIK","VRE 1104",null,"Vypichovač kontaktů ILME-CCFA/CCFD/CCMA/CCMD/CQES, HTS-HE, Harting-0933000, Contact-H-HBO2,5mm","1ks",35.62799915383502,{"$f":"F6120*(1-Elteq!$F$9)","v":35.62799915383502},""]
["TECHNIK","VRE 1204",null,"Vypichovač kontaktů Wieland-SUN Serengeti kontakty","1ks",70.69931082089137,{"$f":"F6121*(1-Elteq!$F$9)","v":70.69931082089137},""]
["TECHNIK","VRE kufr",null,"Prázdný kufr k uložení 4ks vypichovačů","1ks",21.525249488775323,{"$f":"F6122*(1-Elteq!$F$9)","v":21.525249488775323},""]
["TECHNIK","BENNING kabely 2",null,"Bezpečnostní měřící kabely průměr 4mm s hrotem 2mm","1ks",14.473874656245476,{"$f":"F6123*(1-Elteq!$F$9)","v":14.473874656245476},""]
["TECHNIK","BENNING kabely 4",null,"Bezpečnostní měřící kabely průměr 4mm s hrotem 4mm","1ks",20.040749524032197,{"$f":"F6124*(1-Elteq!$F$9)","v":20.040749524032197},""]
["TECHNIK","BENNING pouzdro I",null,"Pouzdro na zkoušečky Benning DUSPOL, starý model","1ks",18.185124568103291,{"$f":"F6125*(1-Elteq!$F$9)","v":18.185124568103291},"4014651109100"]
["TECHNIK","BENNING pouzdro II",null,"Pouzdro na zkoušečky Benning DUSPOL, nový model","1ks",20.411874515217981,{"$f":"F6126*(1-Elteq!$F$9)","v":20.411874515217981},"4014651109117"]
["TECHNIK","CM 1",null,"Klešťový multimetr pro střídavý proud, napětí a odpor","1ks",83.503123016800828,{"$f":"F6127*(1-Elteq!$F$9)","v":83.503123016800828},"4014651000803"]
["TECHNIK","CM 1-1",null,"Klešťový multimetr AC 10mA-400A, rozevření čelistí 30mm","1ks",69.400373351741138,{"$f":"F6128*(1-Elteq!$F$9)","v":69.400373351741138},"4014650440617"]
["TECHNIK","CM 1-2",null,"Klešťový multimetr AC 0,1V-600V / 0,1A-400A / DC 0,1V-600V / 0,1Ω-20MΩ  rozevření čelistí 30mm","1ks",92.59568530085248,{"$f":"F6129*(1-Elteq!$F$9)","v":92.59568530085248},"4014650440624"]
["TECHNIK","CM 1-3",null,"Klešťový multimetr","1ks",124.51243454282968,{"$f":"F6130*(1-Elteq!$F$9)","v":124.51243454282968},"4014650440631"]
["TECHNIK","CM 2",null,"Klešťový multimetr pro stejnosm. a střídavý proud","1ks",198.55187028439309,{"$f":"F6131*(1-Elteq!$F$9)","v":198.55187028439309},"4014651000810"]
["TECHNIK","CM 3",null,"Klešťový multimetr pro střídavý proud","1ks",168.3051835027519,{"$f":"F6132*(1-Elteq!$F$9)","v":168.3051835027519},"4014651000612"]
["TECHNIK","CM 4",null,"Klešťový multimetr pro střídavý proud","1ks",155.50137130684243,{"$f":"F6133*(1-Elteq!$F$9)","v":155.50137130684243},"4014651440562"]
["TECHNIK","CM 5",null,"Klešťový multimetr pro stejnosm. a střídavý proud, napětí, odpor a frekvence","1ks",161.43937116581495,{"$f":"F6134*(1-Elteq!$F$9)","v":161.43937116581495},""]
["TECHNIK","CM 5-1",null,"Klešťový multimetr pro stejnosměrný a střídavý proud","1ks",287.06518068220197,{"$f":"F6135*(1-Elteq!$F$9)","v":287.06518068220197},"4014651440661"]
["TECHNIK","CM 6",null,"Klešťový multimetr pro střídavý proud","1ks",213.39686993182434,{"$f":"F6136*(1-Elteq!$F$9)","v":213.39686993182434},"4014651440586"]
["TECHNIK","CM 7",null,"Klešťový multimetr pro stejnosm. a střídavý proud","1ks",308.77599266657018,{"$f":"F6137*(1-Elteq!$F$9)","v":308.77599266657018},"4014651440593"]
["TECHNIK","CM 8",null,"Klešťový multimetr AC/DC 10mV-1000V / 0,1A-600A / 0,1Ω-20kΩ / 0,11Hz-400Hz / 1W-600kW rozevření 40mm","1ks",338.2804294658398,{"$f":"F6138*(1-Elteq!$F$9)","v":338.2804294658398},"4014650440648"]
["TECHNIK","CM 9",null,"Klešťový digitální multimetr AC 1ųA-100A rozevření čelistí 40mm","1ks",456.48373915851118,{"$f":"F6139*(1-Elteq!$F$9)","v":456.48373915851118},"4014650440655"]
["TECHNIK","DUSPOL analog",null,"Zkoušečka napětí AC 12-1000V, DC 12-1000V, LED/LCD/vibrace, točivé pole, fáze, polarita","1ks",54.740936199902762,{"$f":"F6140*(1-Elteq!$F$9)","v":54.740936199902762},"4014650502611"]
["TECHNIK","DUSPOL combi",null,"Zkoušečka napětí AC 12-400V, DC 12-750V, 0Ω-600kΩ, LED/LCD/vibrace, fáze, polarita","1ks",49.545186323301827,{"$f":"F6141*(1-Elteq!$F$9)","v":49.545186323301827},"4014651502543"]
["TECHNIK","DUSPOL digital",null,"Zkoušečka napětí AC 6-690V, DC 6-750V, 0Ω-200kΩ, LED/LCD/vibrace/bzučák, točivé pole, fáze, polarita","1ks",98.533685159824984,{"$f":"F6142*(1-Elteq!$F$9)","v":98.533685159824984},"4014650502635"]
["TECHNIK","DUSPOL expert",null,"Zkoušečka napětí AC/DC 12-1000V, 0,1-100kO, LED/vibrace, točivé pole, akustická signalizace, CAT IV","1ks",64.761310961918866,{"$f":"F6143*(1-Elteq!$F$9)","v":64.761310961918866},"4014651502628"]
["TECHNIK","DUSPOL master",null,"Zkoušečka napětí AC 12-690V, DC 12-750V, LED/vibrace, točivé pole, fáze, polarita","1ks",43.978311455515104,{"$f":"F6144*(1-Elteq!$F$9)","v":43.978311455515104},"4014651502529"]
["TECHNIK","DUTEST PRO",null,"Zkoušečka průchodnosti vedení 6-400V / indikace odporu 0-100 Ohm, 1 kOhm, 10 kOhm, bzučák","1ks",32.844561719941659,{"$f":"F6145*(1-Elteq!$F$9)","v":32.844561719941659},""]
["TECHNIK","FLUKE 2042",null,"Souprava pro hledání kabelů","1ks",894.04010376654753,{"$f":"F6146*(1-Elteq!$F$9)","v":894.04010376654753},""]
["TECHNIK","FLUKE T110",null,"Zkoušečka napětí 12-690 V AC/DC","1ks",97.976997673046299,{"$f":"F6147*(1-Elteq!$F$9)","v":97.976997673046299},""]
["TECHNIK","FLUKE T130",null,"Zkoušečka napětí do 690 V, propojení a indikátor třífázového točivého pole","1ks",146.96549650956945,{"$f":"F6148*(1-Elteq!$F$9)","v":146.96549650956945},""]
["TECHNIK","FLUKE T150",null,"Zkoušečka napětí do 690 V","1ks",171.45974592783102,{"$f":"F6149*(1-Elteq!$F$9)","v":171.45974592783102},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"IT 120 - CC 2",null,"Proudový klešťový nástavec k IT 120","1ks",140.65637165941118,{"$f":"F6150*(1-Elteq!$F$9)","v":140.65637165941118},"4014650441102"]
["TECHNIK","IT 120 - Luxmetr B",null,"Senzor intenzity osvětlení Luxmetr typ B k IT 120","1ks",298.75561790455407,{"$f":"F6151*(1-Elteq!$F$9)","v":298.75561790455407},"4014650441119"]
["TECHNIK","IT 120 - Uzemnění",null,"Uzemňovací souprava k IT 120","1ks",108.36849742624818,{"$f":"F6152*(1-Elteq!$F$9)","v":108.36849742624818},"4014650441133"]
["TECHNIK","IT 120B",null,"Bezpečnostní, instalační měřicí kontrolní přístroj","1ks",1439.7794033052392,{"$f":"F6153*(1-Elteq!$F$9)","v":1439.7794033052392},"4014651441026"]
["TECHNIK","MM 1",null,"Digitální multimetr s automat. přepínáním rozsahů","1ks",88.51331039780888,{"$f":"F6154*(1-Elteq!$F$9)","v":88.51331039780888},"4014651000513"]
["TECHNIK","MM 1-1",null,"Digitální multimetr MM 1-1","1ks",74.410560732749175,{"$f":"F6155*(1-Elteq!$F$9)","v":74.410560732749175},"4014650440815"]
["TECHNIK","MM 1-2",null,"Digitální multimetr MM 1-2","1ks",93.523497778816932,{"$f":"F6156*(1-Elteq!$F$9)","v":93.523497778816932},"4014650440822"]
["TECHNIK","MM 1-3",null,"Digitální multimetr MM 1-3","1ks",112.26530983369889,{"$f":"F6157*(1-Elteq!$F$9)","v":112.26530983369889},"4014650440839"]
["TECHNIK","MM 2",null,"Digitální multimetr s rozsahem 1000 V","1ks",105.02837250557616,{"$f":"F6158*(1-Elteq!$F$9)","v":105.02837250557616},"4014651000520"]
["TECHNIK","MM 3",null,"Digitální multimetr s měřením kapacity a frekvence","1ks",132.3060593577311,{"$f":"F6159*(1-Elteq!$F$9)","v":132.3060593577311},"4014651000537"]
["TECHNIK","MM 4",null,"Digitální multimetr s klešťovým nástavcem","1ks",151.9756838905775,{"$f":"F6160*(1-Elteq!$F$9)","v":151.9756838905775},"4014651000605"]
["TECHNIK","MM 7-1",null,"Digitální multimetr (náhrada za MM7)","1ks",235.29324441178545,{"$f":"F6161*(1-Elteq!$F$9)","v":235.29324441178545},"4014651440852"]
["TECHNIK","MM 9",null,"Digitální multimetr MM 9","1ks",163.29499612174385,{"$f":"F6162*(1-Elteq!$F$9)","v":163.29499612174385},"4014651440784"]
["TECHNIK","MM P3",null,"Kapesní digitální multimetr","1ks",48.617373845337369,{"$f":"F6163*(1-Elteq!$F$9)","v":48.617373845337369},"4014650440846"]
["TECHNIK","MM10",null,"Digitální multimetr MM 10","1ks",205.9743701081087,{"$f":"F6164*(1-Elteq!$F$9)","v":205.9743701081087},"4014651440791"]
["TECHNIK","MM11",null,"Digitální multimetr MM 11","1ks",438.29861459040791,{"$f":"F6165*(1-Elteq!$F$9)","v":438.29861459040791},"4014651440807"]
["TECHNIK","PROFIPOL",null,"Zkoušečka napětí AC 6-400V, DC 6-400V, LED, polarita","1ks",31.916749241977204,{"$f":"F6166*(1-Elteq!$F$9)","v":31.916749241977204},"4014651000155"]
["TECHNIK","RJT CRONOtester",null,"CRONO tester kabelů RJ-45 / RJ-11 / RJ-12","1ks",6.7544748395812224,{"$f":"F6167*(1-Elteq!$F$9)","v":6.7544748395812224},""]
["TECHNIK","RJT LANtest",null,"LANtest - měřící přístroj k měření správnosti zapojení RJ45, BNC, RJ12, RJ11","1ks",16.329499612174384,{"$f":"F6168*(1-Elteq!$F$9)","v":16.329499612174384},""]
["TECHNIK","RJT TL-828A",null,"Digitální síťový multifunkční kabel tester RJ45","1ks",93.152372787631151,{"$f":"F6169*(1-Elteq!$F$9)","v":93.152372787631151},"8591735053888"]
["TECHNIK","RJT WS-SC8108",null,"Digitální síťový multifunkční kabel tester RJ45","1ks",64.946873457511757,{"$f":"F6170*(1-Elteq!$F$9)","v":64.946873457511757},"8591735053895"]
["TECHNIK","TRITEST eazy",null,"Bezdotyková zkoušečka fází a točivých polí v sítích střídavého proudu","1ks",47.503998871780027,{"$f":"F6171*(1-Elteq!$F$9)","v":47.503998871780027},"4014650200517"]
["TECHNIK","TRITEST PRO",null,"Ukazatel sledu fází s rozsahem napětí 300-50V (50-60Hz) vč. bezpečnostních měřicích hrotů a svorek","1ks",62.905686005989956,{"$f":"F6172*(1-Elteq!$F$9)","v":62.905686005989956},""]
["TECHNIK","VA 1000",null,"Zkoušečka napětí bezkontaktní 50-1000 V se světelnou a akustickou signalizací","1ks",25.830299386530388,{"$f":"F6173*(1-Elteq!$F$9)","v":25.830299386530388},"8591735036775"]
["TECHNIK","Z-TESTER",null,"Číslicový multimetr, zkoušečka náběhu elektroměru","1ks",115.04874726759225,{"$f":"F6174*(1-Elteq!$F$9)","v":115.04874726759225},"4014651000162"]
["TECHNIK","HSe 211",null,"Plochá smršťovací bužírka BROTHER šíře 6mm pro vodiče průměr 1,7-3,2mm, barva bílá, návin 2,1m","1ks",19.112937046067746,{"$f":"F6175*(1-Elteq!$F$9)","v":19.112937046067746},""]
["TECHNIK","HSe 221",null,"Plochá smršťovací bužírka BROTHER šíře 9mm pro vodiče průměr 2,6-5,1mm, barva bílá, návin 2,1m","1ks",20.968562001996652,{"$f":"F6176*(1-Elteq!$F$9)","v":20.968562001996652},""]
["TECHNIK","HSe 231",null,"Plochá smršťovací bužírka BROTHER šíře 12mm pro vodiče průměr 3,6-7,0mm, barva bílá, návin 2,1m","1ks",23.009749453518449,{"$f":"F6177*(1-Elteq!$F$9)","v":23.009749453518449},""]
["TECHNIK","HSe 241",null,"Plochá smršťovací bužírka BROTHER šíře 18mm pro vodiče průměr 5,4-10,6mm, barva bílá, návin 2,1m","1ks",23.937561931482904,{"$f":"F6178*(1-Elteq!$F$9)","v":23.937561931482904},""]
["TECHNIK","HSe 251",null,"Plochá smršťovací bužírka BROTHER šíře 24mm pro vodiče průměr 7,3-14,3mm, barva bílá, návin 2,1m","1ks",26.349874374190485,{"$f":"F6179*(1-Elteq!$F$9)","v":26.349874374190485},""]
["TECHNIK","TC-201",null,"Páska BROTHER plastová samolepicí šíře 12mm, černý tisk na bílé pásce, návin 7,7m","1ks",16.143937116581494,{"$f":"F6180*(1-Elteq!$F$9)","v":16.143937116581494},""]
["TECHNIK","TC-291",null,"Páska BROTHER plastová samolepicí šíře 9mm, černý tisk na bílé pásce, návin 7,7m","1ks",15.216124638617039,{"$f":"F6181*(1-Elteq!$F$9)","v":15.216124638617039},""]
["TECHNIK","TC-491",null,"Páska BROTHER plastová samolepicí šíře 9mm, černý tisk na červené pásce, návin 7,7m","1ks",15.216124638617039,{"$f":"F6182*(1-Elteq!$F$9)","v":15.216124638617039},""]
["TECHNIK","TC-495",null,"Páska BROTHER plastová samolepicí šíře 9mm, bílý tisk na červené pásce, návin 7,7m","1ks",17.9995620725104,{"$f":"F6183*(1-Elteq!$F$9)","v":17.9995620725104},""]
["TECHNIK","TC-591",null,"Páska BROTHER plastová samolepicí šíře 9mm, černý tisk na modré pásce, návin 7,7m","1ks",15.216124638617039,{"$f":"F6184*(1-Elteq!$F$9)","v":15.216124638617039},""]
["TECHNIK","TC-601",null,"Páska BROTHER plastová samolepicí šíře 12mm, černý tisk na žluté pásce, návin 7,7m","1ks",16.143937116581494,{"$f":"F6185*(1-Elteq!$F$9)","v":16.143937116581494},""]
["TECHNIK","TC-691",null,"Páska BROTHER plastová samolepicí šíře 9mm, černý tisk na žluté pásce, návin 7,7m","1ks",15.216124638617039,{"$f":"F6186*(1-Elteq!$F$9)","v":15.216124638617039},""]
["TECHNIK","TM-K231",null,"Páska BROTHER plastová samolepicí šíře 12mm, černý tisk na bílé pásce, návin 8m","1ks",9.2781247796445356,{"$f":"F6187*(1-Elteq!$F$9)","v":9.2781247796445356},""]
["TECHNIK","TX 221",null,"Páska BROTHER plastová samolepicí šíře 9mm, černý tisk / bílý podklad","1ks",25.125161903277405,{"$f":"F6188*(1-Elteq!$F$9)","v":25.125161903277405},""]
["TECHNIK","TX 231",null,"Páska BROTHER plastová samolepicí šíře 12mm, černý tisk / bílý podklad","1ks",27.945711836289345,{"$f":"F6189*(1-Elteq!$F$9)","v":27.945711836289345},""]
["TECHNIK","TX 241",null,"Páska BROTHER plastová samolepicí šíře 18mm, černý tisk / bílý podklad","1ks",33.475474204957486,{"$f":"F6190*(1-Elteq!$F$9)","v":33.475474204957486},""]
["TECHNIK","TX 251",null,"Páska BROTHER plastová samolepicí šíře 24mm, černý tisk / bílý podklad","1ks",39.005236573625631,{"$f":"F6191*(1-Elteq!$F$9)","v":39.005236573625631},""]
["TECHNIK","TX 621",null,"Páska BROTHER plastová samolepicí šíře 9mm, černý tisk / žlutý podklad","1ks",25.125161903277405,{"$f":"F6192*(1-Elteq!$F$9)","v":25.125161903277405},""]
["TECHNIK","TX 631",null,"Páska BROTHER plastová samolepicí šíře 12mm, černý tisk / žlutý podklad","1ks",29.05908680984669,{"$f":"F6193*(1-Elteq!$F$9)","v":29.05908680984669},""]
["TECHNIK","TZe 111",null,"Páska BROTHER plastová laminovaná šíře 6mm, černý tisk na průsvitné pásce, návin 8m","1ks",10.391499753201881,{"$f":"F6194*(1-Elteq!$F$9)","v":10.391499753201881},""]
["TECHNIK","TZe 121",null,"Páska BROTHER plastová laminovaná šíře 9mm, černý tisk na průsvitné pásce, návin 8m","1ks",11.875999717945007,{"$f":"F6195*(1-Elteq!$F$9)","v":11.875999717945007},""]
["TECHNIK","TZe 131",null,"Páska BROTHER plastová laminovaná šíře 12mm, černý tisk na průsvitné pásce, návin 8m","1ks",13.360499682688133,{"$f":"F6196*(1-Elteq!$F$9)","v":13.360499682688133},""]
["TECHNIK","TZe 132",null,"Páska BROTHER plastová laminovaná šíře 12mm, červený tisk na průsvitné pásce, návin 8m","1ks",13.360499682688133,{"$f":"F6197*(1-Elteq!$F$9)","v":13.360499682688133},""]
["TECHNIK","TZe 141",null,"Páska BROTHER plastová laminovaná šíře 18mm, černý tisk na průsvitné pásce, návin 8m","1ks",16.515062107767275,{"$f":"F6198*(1-Elteq!$F$9)","v":16.515062107767275},""]
["TECHNIK","TZe 151",null,"Páska BROTHER plastová laminovaná šíře 24mm, černý tisk na průsvitné pásce, návin 8m","1ks",19.112937046067746,{"$f":"F6199*(1-Elteq!$F$9)","v":19.112937046067746},""]
["TECHNIK","TZe 161",null,"Páska BROTHER plastová laminovaná šíře 36mm, černý tisk na průsvitné pásce, návin 8m","1ks",24.679811913854468,{"$f":"F6200*(1-Elteq!$F$9)","v":24.679811913854468},""]
["TECHNIK","TZe 211",null,"Páska BROTHER plastová laminovaná šíře 6mm, černý tisk na bílé pásce, návin 8m","1ks",11.504874726759224,{"$f":"F6201*(1-Elteq!$F$9)","v":11.504874726759224},""]
["TECHNIK","TZe 211.C",null,"Páska BROTHER kompatibilní plastová laminovaná šíře 6mm, černý tisk na bílé pásce, návin 8m","1ks",6.8658123369369566,{"$f":"F6202*(1-Elteq!$F$9)","v":6.8658123369369566},"8591735053437"]
["TECHNIK","TZe 221",null,"Páska BROTHER plastová laminovaná šíře 9mm, černý tisk na bílé pásce, návin 8m","1ks",12.98937469150235,{"$f":"F6203*(1-Elteq!$F$9)","v":12.98937469150235},""]
["TECHNIK","TZe 221.C",null,"Páska BROTHER kompatibilní plastová laminovaná šíře 9mm, černý tisk na bílé pásce, návin 8m","1ks",7.7936248149014107,{"$f":"F6204*(1-Elteq!$F$9)","v":7.7936248149014107},"8591735053444"]
["TECHNIK","TZe 222",null,"Páska BROTHER plastová laminovaná šíře 9mm, červený tisk na bílé pásce, návin 8m","1ks",13.546062178281023,{"$f":"F6205*(1-Elteq!$F$9)","v":13.546062178281023},""]
["TECHNIK","TZe 231",null,"Páska BROTHER plastová laminovaná šíře 12mm, černý tisk na bílé pásce, návin 8m","1ks",14.473874656245476,{"$f":"F6206*(1-Elteq!$F$9)","v":14.473874656245476},""]
["TECHNIK","TZe 231.C",null,"Páska BROTHER kompatibilní plastová laminovaná šíře 12mm, černý tisk na bílé pásce, návin 8m","1ks",8.1647498060871921,{"$f":"F6207*(1-Elteq!$F$9)","v":8.1647498060871921},"8591735053451"]
["TECHNIK","TZe 241",null,"Páska BROTHER plastová laminovaná šíře 18mm, černý tisk na bílé pásce, návin 8m","1ks",17.071749594545945,{"$f":"F6208*(1-Elteq!$F$9)","v":17.071749594545945},""]
["TECHNIK","TZe 241.C",null,"Páska BROTHER kompatibilní plastová laminovaná šíře 18mm, černý tisk na bílé pásce, návin 8m","1ks",8.9069997884587551,{"$f":"F6209*(1-Elteq!$F$9)","v":8.9069997884587551},"8591735053468"]
["TECHNIK","TZe 251",null,"Páska BROTHER plastová laminovaná šíře 24mm, černý tisk na bílé pásce, návin 8m","1ks",20.040749524032197,{"$f":"F6210*(1-Elteq!$F$9)","v":20.040749524032197},""]
["TECHNIK","TZe 251.C",null,"Páska BROTHER kompatibilní plastová laminovaná šíře 24mm, černý isk na bílé pásce, návin 8m","1ks",11.133749735573444,{"$f":"F6211*(1-Elteq!$F$9)","v":11.133749735573444},"8591735053475"]
["TECHNIK","TZe 261",null,"Páska BROTHER plastová laminovaná šíře 36mm, černý tisk na bílé pásce, návin 8m","1ks",26.349874374190485,{"$f":"F6212*(1-Elteq!$F$9)","v":26.349874374190485},""]
["TECHNIK","TZe 262",null,"Páska BROTHER plastová laminovaná šíře 36mm, červený tisk na bílé pásce, návin 8m","1ks",26.349874374190485,{"$f":"F6213*(1-Elteq!$F$9)","v":26.349874374190485},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"TZe 315",null,"Páska BROTHER plastová laminovaná šíře 6mm, bílý tisk na černé pásce, návin 8m","1ks",14.473874656245476,{"$f":"F6214*(1-Elteq!$F$9)","v":14.473874656245476},""]
["TECHNIK","TZe 325",null,"Páska BROTHER plastová laminovaná šíře 9mm, bílý tisk na černé pásce, návin 8m","1ks",15.958374620988602,{"$f":"F6215*(1-Elteq!$F$9)","v":15.958374620988602},""]
["TECHNIK","TZe 335",null,"Páska BROTHER plastová laminovaná šíře 12mm, bílý tisk na černé pásce, návin 8m","1ks",17.81399957691751,{"$f":"F6216*(1-Elteq!$F$9)","v":17.81399957691751},""]
["TECHNIK","TZe 345",null,"Páska BROTHER plastová laminovaná šíře 18mm, bílý tisk na černé pásce, návin 8m","1ks",20.782999506403762,{"$f":"F6217*(1-Elteq!$F$9)","v":20.782999506403762},""]
["TECHNIK","TZe 355",null,"Páska BROTHER plastová laminovaná šíře 24mm, bílý tisk na černé pásce, návin 8m","1ks",23.751999435890014,{"$f":"F6218*(1-Elteq!$F$9)","v":23.751999435890014},""]
["TECHNIK","TZe 421",null,"Páska BROTHER plastová laminovaná šíře 9mm, černý tisk na červené pásce, návin 8m","1ks",12.98937469150235,{"$f":"F6219*(1-Elteq!$F$9)","v":12.98937469150235},""]
["TECHNIK","TZe 431",null,"Páska BROTHER plastová laminovaná šíře 12mm, černý tisk na červené pásce, návin 8m","1ks",14.473874656245476,{"$f":"F6220*(1-Elteq!$F$9)","v":14.473874656245476},""]
["TECHNIK","TZe 441",null,"Páska BROTHER plastová laminovaná šíře 18mm, černý tisk na červené pásce, návin 8m","1ks",17.071749594545945,{"$f":"F6221*(1-Elteq!$F$9)","v":17.071749594545945},""]
["TECHNIK","TZe 451",null,"Páska BROTHER plastová laminovaná šíře 24mm, černý tisk na červené pásce, návin 8m","1ks",20.782999506403762,{"$f":"F6222*(1-Elteq!$F$9)","v":20.782999506403762},""]
["TECHNIK","TZe 461",null,"Páska BROTHER plastová laminovaná šíře 36mm, černý tisk na červené pásce, návin 8m","1ks",26.349874374190485,{"$f":"F6223*(1-Elteq!$F$9)","v":26.349874374190485},""]
["TECHNIK","TZe 521",null,"Páska BROTHER plastová laminovaná šíře 9mm, černý tisk na modré pásce, návin 8m","1ks",13.546062178281023,{"$f":"F6224*(1-Elteq!$F$9)","v":13.546062178281023},""]
["TECHNIK","TZe 531",null,"Páska BROTHER plastová laminovaná šíře 12mm, černý tisk na modré pásce, návin 8m","1ks",14.473874656245476,{"$f":"F6225*(1-Elteq!$F$9)","v":14.473874656245476},""]
["TECHNIK","TZe 535",null,"Páska BROTHER plastová laminovaná šíře 12mm, bílý tisk na modré pásce, návin 8m","1ks",17.81399957691751,{"$f":"F6226*(1-Elteq!$F$9)","v":17.81399957691751},""]
["TECHNIK","TZe 551",null,"Páska BROTHER plastová laminovaná šíře 24mm, černý tisk na modré pásce, návin 8m","1ks",20.782999506403762,{"$f":"F6227*(1-Elteq!$F$9)","v":20.782999506403762},""]
["TECHNIK","TZe 611",null,"Páska BROTHER plastová laminovaná šíře 6mm, černý tisk na žluté pásce, návin 8m","1ks",11.875999717945007,{"$f":"F6228*(1-Elteq!$F$9)","v":11.875999717945007},""]
["TECHNIK","TZe 611.C",null,"Páska BROTHER kompatibilní plastová laminovaná šíře 6mm, černý tisk na žluté pásce, návin 8m","1ks",6.8658123369369566,{"$f":"F6229*(1-Elteq!$F$9)","v":6.8658123369369566},"8591735053482"]
["TECHNIK","TZe 621",null,"Páska BROTHER plastová laminovaná šíře 9mm, černý tisk na žluté pásce, návin 8m","1ks",12.98937469150235,{"$f":"F6230*(1-Elteq!$F$9)","v":12.98937469150235},""]
["TECHNIK","TZe 621.C",null,"Páska BROTHER kompatibilní plastová laminovaná šíře 9mm, černý tisk na žluté pásce, návin 8m","1ks",7.7936248149014107,{"$f":"F6231*(1-Elteq!$F$9)","v":7.7936248149014107},"8591735053499"]
["TECHNIK","TZe 631",null,"Páska BROTHER plastová laminovaná šíře 12mm, černý tisk na žluté pásce, návin 8m","1ks",14.473874656245476,{"$f":"F6232*(1-Elteq!$F$9)","v":14.473874656245476},""]
["TECHNIK","TZe 631.C",null,"Páska BROTHER kompatibilní plastová laminovaná šíře 12mm, černý tisk na žluté pásce, návin 8m","1ks",8.1647498060871921,{"$f":"F6233*(1-Elteq!$F$9)","v":8.1647498060871921},"8591735053505"]
["TECHNIK","TZe 641",null,"Páska BROTHER plastová laminovaná šíře 18mm, černý tisk na žluté pásce, návin 8m","1ks",17.071749594545945,{"$f":"F6234*(1-Elteq!$F$9)","v":17.071749594545945},""]
["TECHNIK","TZe 641.C",null,"Páska BROTHER kompatibilní plastová laminovaná šíře 18mm, černý tisk na žluté pásce, návin 8m","1ks",8.9069997884587551,{"$f":"F6235*(1-Elteq!$F$9)","v":8.9069997884587551},"8591735053512"]
["TECHNIK","TZe 651",null,"Páska BROTHER plastová laminovaná šíře 24mm, černý tisk na žluté pásce, návin 8m","1ks",20.040749524032197,{"$f":"F6236*(1-Elteq!$F$9)","v":20.040749524032197},""]
["TECHNIK","TZe 651.C",null,"Páska BROTHER kompatibilní plastová laminovaná šíře 24mm, černý tisk na žluté pásce, návin 8m","1ks",11.133749735573444,{"$f":"F6237*(1-Elteq!$F$9)","v":11.133749735573444},"8591735054328"]
["TECHNIK","TZe 661",null,"Páska BROTHER plastová laminovaná šíře 36mm, černý tisk na žluté pásce, návin 8m","1ks",26.349874374190485,{"$f":"F6238*(1-Elteq!$F$9)","v":26.349874374190485},""]
["TECHNIK","TZe 721",null,"Páska BROTHER plastová laminovaná šíře 9mm, černý tisk na zelené pásce, návin 8m","1ks",13.546062178281023,{"$f":"F6239*(1-Elteq!$F$9)","v":13.546062178281023},""]
["TECHNIK","TZe 731",null,"Páska BROTHER plastová laminovaná šíře 12mm, černý tisk na zelené pásce, návin 8m","1ks",14.473874656245476,{"$f":"F6240*(1-Elteq!$F$9)","v":14.473874656245476},""]
["TECHNIK","TZe 741",null,"Páska BROTHER plastová laminovaná šíře 18mm, černý tisk na zelené pásce, návin 8m","1ks",17.81399957691751,{"$f":"F6241*(1-Elteq!$F$9)","v":17.81399957691751},""]
["TECHNIK","TZe B31",null,"Páska BROTHER plastová flexibilní šíře 12mm, černý tisk na signální oranžové pásce","1ks",16.700624603360165,{"$f":"F6242*(1-Elteq!$F$9)","v":16.700624603360165},""]
["TECHNIK","TZe C51",null,"Páska BROTHER plastová laminovaná šíře 24mm, černý tisk na signální žluté pásce","1ks",23.009749453518449,{"$f":"F6243*(1-Elteq!$F$9)","v":23.009749453518449},""]
["TECHNIK","TZe FX231",null,"Páska BROTHER plastová flexibilní šíře 12mm, černý tisk na bílé pásce, návin 8m","1ks",15.958374620988602,{"$f":"F6244*(1-Elteq!$F$9)","v":15.958374620988602},""]
["TECHNIK","TZe FX241",null,"Páska BROTHER plastová flexibilní šíře 18mm, černý tisk na bílé pásce, návin 8m","1ks",18.927374550474855,{"$f":"F6245*(1-Elteq!$F$9)","v":18.927374550474855},""]
["TECHNIK","TZe FX251",null,"Páska BROTHER plastová flexibilní šíře 24mm, černý tisk na bílé pásce, návin 8m","1ks",20.968562001996652,{"$f":"F6246*(1-Elteq!$F$9)","v":20.968562001996652},""]
["TECHNIK","TZe FX621",null,"Páska BROTHER plastová flexibilní šíře 9mm, černý tisk na žluté pásce, návin 8m","1ks",14.844999647431258,{"$f":"F6247*(1-Elteq!$F$9)","v":14.844999647431258},""]
["TECHNIK","TZe FX641",null,"Páska BROTHER plastová flexibilní šíře 18mm, černý tisk na žluté pásce, návin 8m","1ks",18.927374550474855,{"$f":"F6248*(1-Elteq!$F$9)","v":18.927374550474855},""]
["TECHNIK","TZe FX651",null,"Páska BROTHER plastová flexibilní šíře 24mm, černý tisk na žluté pásce, návin 8m","1ks",20.968562001996652,{"$f":"F6249*(1-Elteq!$F$9)","v":20.968562001996652},""]
["TECHNIK","TZe M931",null,"Páska BROTHER plastová laminovaná šíře 12mm, černý tisk na stříbrné pásce, návin 8m","1ks",16.886187098953055,{"$f":"F6250*(1-Elteq!$F$9)","v":16.886187098953055},""]
["TECHNIK","TZe M961",null,"Páska BROTHER plastová laminovaná šíře 36mm, černý tisk na stříbrné pásce, návin 8m","1ks",28.576624321305172,{"$f":"F6251*(1-Elteq!$F$9)","v":28.576624321305172},""]
["TECHNIK","TZe N221",null,"Páska BROTHER plastová nelaminovaná šíře 9mm, černý tisk na bílé pásce, návin 8m","1ks",11.690437222352116,{"$f":"F6252*(1-Elteq!$F$9)","v":11.690437222352116},""]
["TECHNIK","TZe N231",null,"Páska BROTHER plastová nelaminovaná šíře 12mm, černý tisk na bílé pásce, návin 8m","1ks",12.061562213537897,{"$f":"F6253*(1-Elteq!$F$9)","v":12.061562213537897},""]
["TECHNIK","TZe N241",null,"Páska BROTHER plastová nelaminovaná šíře 18mm, černý tisk na bílé pásce, návin 8m","1ks",14.844999647431258,{"$f":"F6254*(1-Elteq!$F$9)","v":14.844999647431258},""]
["TECHNIK","TZe S211",null,"Páska BROTHER extrémně adhesivní šíře 6mm, černý tisk na bílé pásce, návin 8m","1ks",13.546062178281023,{"$f":"F6255*(1-Elteq!$F$9)","v":13.546062178281023},""]
["TECHNIK","TZe S211.C",null,"Páska BROTHER kompatibilní extrémně adhesivní šíře 6mm, černý tisk na bílé pásce, návin 8m","1ks",8.3503123016800824,{"$f":"F6256*(1-Elteq!$F$9)","v":8.3503123016800824},"8591735053611"]
["TECHNIK","TZe S221",null,"Páska BROTHER extrémně adhesivní šíře 9mm, černý tisk na bílé pásce, návin 8m","1ks",14.659437151838368,{"$f":"F6257*(1-Elteq!$F$9)","v":14.659437151838368},""]
["TECHNIK","TZe S221.C",null,"Páska BROTHER kompatibilní extrémně adhesivní šíře 9mm, černý tisk na bílé pásce, návin 8m","1ks",8.3503123016800824,{"$f":"F6258*(1-Elteq!$F$9)","v":8.3503123016800824},"8591735053628"]
["TECHNIK","TZe S231",null,"Páska BROTHER extrémně adhesivní šíře 12mm, černý tisk na bílé pásce, návin 8m","1ks",16.329499612174384,{"$f":"F6259*(1-Elteq!$F$9)","v":16.329499612174384},""]
["TECHNIK","TZe S231.C",null,"Páska BROTHER kompatibilní extrémně adhesivní šíře 12mm, černý tisk na bílé pásce, návin 8m","1ks",8.3503123016800824,{"$f":"F6260*(1-Elteq!$F$9)","v":8.3503123016800824},""]
["TECHNIK","TZe S241",null,"Páska BROTHER extrémně adhesivní šíře 18mm, černý tisk na bílé pásce, návin 8m","1ks",18.927374550474855,{"$f":"F6261*(1-Elteq!$F$9)","v":18.927374550474855},""]
["TECHNIK","TZe S241.C",null,"Páska BROTHER kompatibilní extrémně adhesivní šíře 18mm, černý tisk na bílé pásce, návin 8m","1ks",10.391499753201881,{"$f":"F6262*(1-Elteq!$F$9)","v":10.391499753201881},"8591735053635"]
["TECHNIK","TZe S251",null,"Páska BROTHER extrémně adhesivní šíře 24mm, černý tisk na bílé pásce, návin 8m","1ks",21.525249488775323,{"$f":"F6263*(1-Elteq!$F$9)","v":21.525249488775323},""]
["TECHNIK","TZe S251.C",null,"Páska BROTHER kompatibilní extrémně adhesivní šíře 24mm, černý tisk na bílé pásce, návin 8m","1ks",11.875999717945007,{"$f":"F6264*(1-Elteq!$F$9)","v":11.875999717945007},"8591735053642"]
["TECHNIK","TZe S261",null,"Páska BROTHER extrémně adhesivní šíře 36mm, černý tisk na bílé pásce, návin 8m","1ks",28.391061825712281,{"$f":"F6265*(1-Elteq!$F$9)","v":28.391061825712281},""]
["TECHNIK","TZe S261.C",null,"Páska BROTHER kompatibilní extrémně adhesivní šíře 36mm, černý tisk na bílé pásce, návin 8m","1ks",15.030562143024149,{"$f":"F6266*(1-Elteq!$F$9)","v":15.030562143024149},"8591735053659"]
["TECHNIK","TZe S611.C",null,"Páska BROTHER kompatibilní extrémně adhesivní šíře 6mm, černý tisk na žluté pásce, návin 8m","1ks",8.3503123016800824,{"$f":"F6267*(1-Elteq!$F$9)","v":8.3503123016800824},""]
["TECHNIK","TZe S621",null,"Páska BROTHER extrémně adhesivní šíře 9mm, černý tisk na žluté pásce, návin 8m","1ks",14.659437151838368,{"$f":"F6268*(1-Elteq!$F$9)","v":14.659437151838368},""]
["TECHNIK","TZe S631",null,"Páska BROTHER extrémně adhesivní šíře 12mm, černý tisk na žluté pásce, návin 8m","1ks",16.329499612174384,{"$f":"F6269*(1-Elteq!$F$9)","v":16.329499612174384},""]
["TECHNIK","TZe S641",null,"Páska BROTHER extrémně adhesivní šíře 18mm, černý tisk na žluté pásce, návin 8m","1ks",18.927374550474855,{"$f":"F6270*(1-Elteq!$F$9)","v":18.927374550474855},""]
["TECHNIK","TZe S651",null,"Páska BROTHER extrémně adhesivní šíře 24mm, černý tisk na žluté pásce, návin 8m","1ks",21.525249488775323,{"$f":"F6271*(1-Elteq!$F$9)","v":21.525249488775323},""]
["TECHNIK","TZe SE4",null,"Páska BROTHER laminovaná plombovací šíře 18mm, bílý tisk na černé pásce, návin 8m","1ks",28.762186816898062,{"$f":"F6272*(1-Elteq!$F$9)","v":28.762186816898062},""]
["TECHNIK","DK 11208",null,"Štítky BROTHER adresní široké bílé rozměr 38x90mm pro tiskárny QL","400ks",12.80381219590946,{"$f":"F6273*(1-Elteq!$F$9)","v":12.80381219590946},""]
["TECHNIK","DK 11241",null,"Štítky BROTHER poštovní velké bílé rozměr 102x152mm pro tiskárny QL","200ks",32.844561719941659,{"$f":"F6274*(1-Elteq!$F$9)","v":32.844561719941659},""]
["TECHNIK","DK 22212",null,"Štítky BROTHER kontinuální role pro tiskárny QL","1ks",42.679373986364865,{"$f":"F6275*(1-Elteq!$F$9)","v":42.679373986364865},""]
["TECHNIK","DK 22606",null,"Štítky BROTHER kontinuální role pro tiskárny QL","1ks",60.493373563282375,{"$f":"F6276*(1-Elteq!$F$9)","v":60.493373563282375},""]
["TECHNIK","AD-24ESEU",null,"Síťový adaptér pro štítkovače BROTHER 7,0-9,5V / 1,3A","1ks",15.401687134209931,{"$f":"F6277*(1-Elteq!$F$9)","v":15.401687134209931},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"AD-E001",null,"Síťový adaptér pro štítkovače BROTHER 12V / 2,0A","1ks",19.484062037253526,{"$f":"F6278*(1-Elteq!$F$9)","v":19.484062037253526},""]
["TECHNIK","BA-7000",null,"Náhradní bateriový blok pro elektronický štítkovač BROTHER PT-7600","1ks",41.009311526028853,{"$f":"F6279*(1-Elteq!$F$9)","v":41.009311526028853},""]
["TECHNIK","BA-E001",null,"Náhradní bateriový blok Li-Ion pro elektronické štítkovače PT","1ks",24.123124427075794,{"$f":"F6280*(1-Elteq!$F$9)","v":24.123124427075794},""]
["TECHNIK","PT-3600",null,"Elektronický štítkovač BROTHER pro pásky TZe šíře 6 - 36mm, USB, stolní model","1ks",381.88761593016915,{"$f":"F6281*(1-Elteq!$F$9)","v":381.88761593016915},""]
["TECHNIK","PT-9600 + kufr",null,"Elektronický štítkovač BROTHER pro pásky TZe šíře 6 - 36mm, USB, stolní model + kufr","1ks",617.9231103243261,{"$f":"F6282*(1-Elteq!$F$9)","v":617.9231103243261},""]
["TECHNIK","PT-9700 PC",null,"Elektronický štítkovač BROTHER pro pásky TZe šíře 6 - 36mm, USB, stolní model, profi","1ks",343.66174183803361,{"$f":"F6283*(1-Elteq!$F$9)","v":343.66174183803361},""]
["TECHNIK","PT-9800PCN",null,"Elektronický štítkovač BROTHER pro pásky TZe šíře 6 - 36mm, USB, stolní model + adaptér 220V","1ks",573.75923637321819,{"$f":"F6284*(1-Elteq!$F$9)","v":573.75923637321819},""]
["TECHNIK","PT-D200 BW",null,"Elektronický štítkovač BROTHER pro pásky TZe šíře 6 - 12mm, stolní model","1ks",45.462811420258227,{"$f":"F6285*(1-Elteq!$F$9)","v":45.462811420258227},""]
["TECHNIK","PT-D200 BW VP",null,"Elektronický štítkovač BROTHER pro pásky TZe šíře 6 - 12mm, stolní model + adaptér 220V, kufr","1ks",63.276810997175737,{"$f":"F6286*(1-Elteq!$F$9)","v":63.276810997175737},""]
["TECHNIK","PT-D200 VP",null,"Elektronický štítkovač BROTHER pro pásky TZe šíře 6 - 12mm, stolní model + kufr, adaptér 220V","1ks",58.637748607353473,{"$f":"F6287*(1-Elteq!$F$9)","v":58.637748607353473},""]
["TECHNIK","PT-D450 VP",null,"Elektronický štítkovač BROTHER pro pásky TZe šíře 6 - 18mm, USB, stolní model + adaptér 220V, kufr","1ks",111.52305985132733,{"$f":"F6288*(1-Elteq!$F$9)","v":111.52305985132733},""]
["TECHNIK","PT-D600 VP",null,"Elektronický štítkovač BROTHER pro pásky TZe šíře 6 - 24mm, USB, stolní model + adaptér 220V, kufr","1ks",148.07887148312679,{"$f":"F6289*(1-Elteq!$F$9)","v":148.07887148312679},""]
["TECHNIK","PT-E100 VP+kufr",null,"Elektronický štítkovač BROTHER pro pásky TZe šíře 6 - 12mm, ruční model + adaptér 220V, kufr","1ks",56.225436164645892,{"$f":"F6290*(1-Elteq!$F$9)","v":56.225436164645892},""]
["TECHNIK","PT-E300 VP+kufr",null,"Elektronický štítkovač BROTHER pro pásky TZe šíře 6 - 18mm, také pro smršťovací bužírky + kufr","1ks",136.94512174755337,{"$f":"F6291*(1-Elteq!$F$9)","v":136.94512174755337},""]
["TECHNIK","PT-E550WVP+kufr AKCE",null,"Elektronický štítkovač BROTHER pro pásky TZe šíře 6 - 24mm, USB, WiFi + adaptér 220V, kufr, +4 pásky","1ks",229.16968205722006,{"$f":"F6292*(1-Elteq!$F$9)","v":229.16968205722006},""]
["TECHNIK","PT-H105 WB",null,"Elektronický štítkovač BROTHER pro pásky TZe šíře 6 - 12mm, ruční model","1ks",39.710374056878614,{"$f":"F6293*(1-Elteq!$F$9)","v":39.710374056878614},""]
["TECHNIK","PT-H300",null,"Elektronický štítkovač BROTHER pro pásky TZe šíře 6 - 18mm, ruční model","1ks",74.224998237156285,{"$f":"F6294*(1-Elteq!$F$9)","v":74.224998237156285},""]
["TECHNIK","PT-H500",null,"Elektronický štítkovač BROTHER pro pásky TZe šíře 6 - 24mm, USB, ruční model","1ks",123.02793457808656,{"$f":"F6295*(1-Elteq!$F$9)","v":123.02793457808656},""]
["TECHNIK","PT-P700",null,"Elektronický štítkovač BROTHER pro pásky TZe šíře 6 - 24mm, USB, stolní model + adaptér 220V","1ks",98.162560168639189,{"$f":"F6296*(1-Elteq!$F$9)","v":98.162560168639189},""]
["TECHNIK","PT-P750 W",null,"Elektronický štítkovač BROTHER pro pásky TZe šíře 6 - 24mm, USB, stolní model + adaptér 220V","1ks",161.43937116581495,{"$f":"F6297*(1-Elteq!$F$9)","v":161.43937116581495},""]
["TECHNIK","QL 1050",null,"Elektronická tiskárna štítků BROTHER pro papírové a plastové pásky a etikety DK","1ks",249.76711906803092,{"$f":"F6298*(1-Elteq!$F$9)","v":249.76711906803092},""]
["TECHNIK","QL 1060 N",null,"Elektronická tiskárna štítků BROTHER pro papírové a plastové pásky a etikety DK","1ks",303.39468029437631,{"$f":"F6299*(1-Elteq!$F$9)","v":303.39468029437631},""]
["TECHNIK","QL 570",null,"Elektronická tiskárna štítků BROTHER pro papírové a plastové pásky a etikety DK","1ks",98.162560168639189,{"$f":"F6300*(1-Elteq!$F$9)","v":98.162560168639189},""]
["TECHNIK","QL 650 TD",null,"Elektronická tiskárna štítků BROTHER pro papírové a plastové pásky a etikety DK","1ks",209.31449502878075,{"$f":"F6301*(1-Elteq!$F$9)","v":209.31449502878075},""]
["TECHNIK","QL 700",null,"Elektronická tiskárna štítků BROTHER pro papírové a plastové pásky a etikety DK","1ks",123.02793457808656,{"$f":"F6302*(1-Elteq!$F$9)","v":123.02793457808656},""]
["TECHNIK","QL 710 W",null,"Elektronická tiskárna štítků BROTHER pro papírové a plastové pásky a etikety DK","1ks",161.43937116581495,{"$f":"F6303*(1-Elteq!$F$9)","v":161.43937116581495},""]
["TECHNIK","QL 720 NW",null,"Elektronická tiskárna štítků BROTHER pro papírové a plastové pásky a etikety DK","1ks",194.09837039016369,{"$f":"F6304*(1-Elteq!$F$9)","v":194.09837039016369},""]
["TECHNIK","M-1 SB bílá 3,2/1,6",null,"3476A079 kazeta se smršťovací bužírkou 3,2/1,6mm, návin 5m, barva bílá","1ks",33.40124920672033,{"$f":"F6305*(1-Elteq!$F$9)","v":33.40124920672033},"8591735020521"]
["TECHNIK","M-1 SB bílá 3/1",null,"3476A085 kazeta se smršťovací bužírkou 3,0/1,0mm, návin 5m, barva bílá","1ks",46.019498907036898,{"$f":"F6306*(1-Elteq!$F$9)","v":46.019498907036898},"8591735020538"]
["TECHNIK","M-1 SB bílá 4,8/2,4",null,"3476A081 kazeta se smršťovací bužírkou 4,8/2,4mm, návin 5m, barva bílá","1ks",36.184686640613691,{"$f":"F6307*(1-Elteq!$F$9)","v":36.184686640613691},"8591735020545"]
["TECHNIK","M-1 SB bílá 6,4/3,2",null,"3476A083 kazeta se smršťovací bužírkou 6,4/3,2mm, návin 5m, barva bílá","1ks",43.421623968736434,{"$f":"F6308*(1-Elteq!$F$9)","v":43.421623968736434},"8591735020552"]
["TECHNIK","M-1 SB bílá 6/2",null,"3476A087 kazeta se smršťovací bužírkou 6,0/2,0mm, návin 5m, barva bílá","1ks",54.184248713124092,{"$f":"F6309*(1-Elteq!$F$9)","v":54.184248713124092},"8591735020569"]
["TECHNIK","M-1 SB žlutá 3,2/1,6",null,"3476A080 kazeta se smršťovací bužírkou 3,2/1,6mm, návin 5m, barva žlutá","1ks",33.40124920672033,{"$f":"F6310*(1-Elteq!$F$9)","v":33.40124920672033},"8591735020576"]
["TECHNIK","M-1 SB žlutá 3/1",null,"3476A086 kazeta se smršťovací bužírkou 3,0/1,0mm, návin 5m, barva žlutá","1ks",46.019498907036898,{"$f":"F6311*(1-Elteq!$F$9)","v":46.019498907036898},"8591735020583"]
["TECHNIK","M-1 SB žlutá 4,8/2,4",null,"3476A082 kazeta se smršťovací bužírkou 4,8/2,4mm, návin 5m, barva žlutá","1ks",36.184686640613691,{"$f":"F6312*(1-Elteq!$F$9)","v":36.184686640613691},"8591735020590"]
["TECHNIK","M-1 SB žlutá 6,4/3,2",null,"3476A084 kazeta se smršťovací bužírkou 6,4/3,2mm, návin 5m, barva žlutá","1ks",43.421623968736434,{"$f":"F6313*(1-Elteq!$F$9)","v":43.421623968736434},"8591735020606"]
["TECHNIK","M-1 SB žlutá 6/2",null,"3476A088 kazeta se smršťovací bužírkou 6,0/2,0mm, návin 5m, barva žlutá","1ks",54.184248713124092,{"$f":"F6314*(1-Elteq!$F$9)","v":54.184248713124092},"8591735020613"]
["TECHNIK","LK330 PÁS 6 bílá",null,"Samolepicí páska pro tiskárnu LK330, návin 8m, šíře 6mm, barva bílá (LM406WL)","1ks",17.44287458573173,{"$f":"F6315*(1-Elteq!$F$9)","v":17.44287458573173},""]
["TECHNIK","LK330 PÁS 6 stříbrná",null,"Samolepicí páska pro tiskárnu LK330, návin 8m, šíře 6mm, barva stříbrná (LM406SL)","1ks",17.44287458573173,{"$f":"F6316*(1-Elteq!$F$9)","v":17.44287458573173},""]
["TECHNIK","LK330 PÁS 6 žlutá",null,"Samolepicí páska pro tiskárnu LK330, návin 8m, šíře 6mm, barva žlutá (LM406YL)","1ks",17.44287458573173,{"$f":"F6317*(1-Elteq!$F$9)","v":17.44287458573173},""]
["TECHNIK","LK330 PÁS 9 bílá",null,"Samolepicí páska pro tiskárnu LK330, návin 8m, šíře 9mm, barva bílá (LM409WL)","1ks",17.44287458573173,{"$f":"F6318*(1-Elteq!$F$9)","v":17.44287458573173},""]
["TECHNIK","LK330 PÁS 9 stříbrná",null,"Samolepicí páska pro tiskárnu LK330, návin 8m, šíře 9mm, barva stříbrná (LM409SL)","1ks",17.44287458573173,{"$f":"F6319*(1-Elteq!$F$9)","v":17.44287458573173},""]
["TECHNIK","LK330 PÁS 9 žlutá",null,"Samolepicí páska pro tiskárnu LK330, návin 8m, šíře 9mm, barva žlutá (LM409YL)","1ks",17.44287458573173,{"$f":"F6320*(1-Elteq!$F$9)","v":17.44287458573173},""]
["TECHNIK","LK330 PÁS12 bílá",null,"Samolepicí páska pro tiskárnu LK330, návin 8m, šíře 12mm, barva bílá (LM412WL)","1ks",17.44287458573173,{"$f":"F6321*(1-Elteq!$F$9)","v":17.44287458573173},""]
["TECHNIK","LK330 PÁS12 stříbrná",null,"Samolepicí páska pro tiskárnu LK330, návin 8m, šíře 12mm, barva stříbrná (LM412SL)","1ks",17.44287458573173,{"$f":"F6322*(1-Elteq!$F$9)","v":17.44287458573173},""]
["TECHNIK","LK330 PÁS12 žlutá",null,"Samolepicí páska pro tiskárnu LK330, návin 8m, šíře 12mm, barva žlutá (LM412YL)","1ks",17.44287458573173,{"$f":"F6323*(1-Elteq!$F$9)","v":17.44287458573173},""]
["TECHNIK","LK330 TISK černá",null,"Tisková páska pro tiskárnu L-MARK model LK-330, návin 80m, barva černá","1ks",27.092124356562046,{"$f":"F6324*(1-Elteq!$F$9)","v":27.092124356562046},"8591735040949"]
["TECHNIK","M-1 NN  6 bílá",null,"Náhradní náplň do kazety se samolepicí páskou, šíře 6mm, návin 30m, barva bílá","1ks",36.741374127392362,{"$f":"F6325*(1-Elteq!$F$9)","v":36.741374127392362},"8591735020415"]
["TECHNIK","M-1 NN  6 stříbrná",null,"Náhradní náplň do kazety se samolepicí páskou, šíře 6mm, návin 30m, barva stříbrná","1ks",36.741374127392362,{"$f":"F6326*(1-Elteq!$F$9)","v":36.741374127392362},"8591735046309"]
["TECHNIK","M-1 NN  6 žlutá",null,"Náhradní náplň do kazety se samolepicí páskou, šíře 6mm, návin 30m, barva žlutá","1ks",36.741374127392362,{"$f":"F6327*(1-Elteq!$F$9)","v":36.741374127392362},"8591735020422"]
["TECHNIK","M-1 NN  9 bílá",null,"Náhradní náplň do kazety se samolepicí páskou, šíře 9mm, návin 30m, barva bílá","1ks",51.58637377482362,{"$f":"F6328*(1-Elteq!$F$9)","v":51.58637377482362},"8591735020439"]
["TECHNIK","M-1 NN  9 stříbrná",null,"Náhradní náplň do kazety se samolepicí páskou, šíře 9mm, návin 30m, barva stříbrná","1ks",51.58637377482362,{"$f":"F6329*(1-Elteq!$F$9)","v":51.58637377482362},"8591735046323"]
["TECHNIK","M-1 NN  9 žlutá",null,"Náhradní náplň do kazety se samolepicí páskou, šíře 9mm, návin 30m, barva žlutá","1ks",51.58637377482362,{"$f":"F6330*(1-Elteq!$F$9)","v":51.58637377482362},"8591735020446"]
["TECHNIK","M-1 NN 12 bílá",null,"Náhradní náplň do kazety se samolepicí páskou, šíře 12mm, návin 30m, barva bílá","1ks",66.060248431069098,{"$f":"F6331*(1-Elteq!$F$9)","v":66.060248431069098},"8591735020453"]
["TECHNIK","M-1 NN 12 stříbrná",null,"Náhradní náplň do kazety se samolepicí páskou, šíře 12mm, návin 30m, barva stříbrná","1ks",66.060248431069098,{"$f":"F6332*(1-Elteq!$F$9)","v":66.060248431069098},"8591735046330"]
["TECHNIK","M-1 NN 12 žlutá",null,"Náhradní náplň do kazety se samolepicí páskou, šíře 12mm, návin 30m, barva žlutá","1ks",66.060248431069098,{"$f":"F6333*(1-Elteq!$F$9)","v":66.060248431069098},"8591735020460"]
["TECHNIK","M-1 OBM-PÁSKA",null,"3476A075 kazeta s obmotávací páskou, šíře 12mm, návin 8m, barva bílá","1ks",71.441560803262931,{"$f":"F6334*(1-Elteq!$F$9)","v":71.441560803262931},"8591735048525"]
["TECHNIK","M-1 OBM-PÁSKA 33",null,"3476A075 kazeta s obmotávací páskou, šíře 33mm, návin 8m, barva bílá","1ks",91.667872822888015,{"$f":"F6335*(1-Elteq!$F$9)","v":91.667872822888015},""]
["TECHNIK","M-1 PÁSEK  4 bílá",null,"3476A035 kazeta s plastovým páskem ID STRIP, šíře 4mm, návin 5m, barva bílá","1ks",16.515062107767275,{"$f":"F6336*(1-Elteq!$F$9)","v":16.515062107767275},"8591735016296"]
["TECHNIK","M-1 PÁSEK  4 žlutá",null,"3476A075 kazeta s plastovým páskem ID STRIP, šíře 4mm, návin 5m, barva žlutá","1ks",16.515062107767275,{"$f":"F6337*(1-Elteq!$F$9)","v":16.515062107767275},"8591735020484"]
["TECHNIK","M-1 PÁSEK  9 bílá",null,"3476A036 kazeta s plastovým páskem ID STRIP, šíře 9mm, návin 5m, barva bílá","1ks",17.81399957691751,{"$f":"F6338*(1-Elteq!$F$9)","v":17.81399957691751},"8591735051129"]
["TECHNIK","M-1 PÁSEK  9 žlutá",null,"3476A076 kazeta s plastovým páskem ID STRIP, šíře 9mm, návin 5m, barva žlutá","1ks",17.81399957691751,{"$f":"F6339*(1-Elteq!$F$9)","v":17.81399957691751},"8591735051136"]
["TECHNIK","M-1 PÁSEK 12 bílá",null,"3476A037 kazeta s plastovým páskem ID STRIP, šíře 12mm, návin 5m, barva bílá","1ks",20.226312019625091,{"$f":"F6340*(1-Elteq!$F$9)","v":20.226312019625091},"8591735051143"]
["TECHNIK","M-1 PÁSEK 12 žlutá",null,"3476A077 kazeta s plastovým páskem ID STRIP, šíře 12mm, návin 5m, barva žlutá","1ks",20.226312019625091,{"$f":"F6341*(1-Elteq!$F$9)","v":20.226312019625091},"8591735051150"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"M-1 PÁSKA  6 bílá",null,"3476A023 kazeta se samolepicí páskou, šíře 6mm, návin 30m, barva bílá","1ks",57.524373633796124,{"$f":"F6342*(1-Elteq!$F$9)","v":57.524373633796124},"8591735016333"]
["TECHNIK","M-1 PÁSKA  6 stříbr.",null,"3476A068 kazeta se samolepicí páskou, šíře 6mm, návin 27m, barva stříbrná","1ks",64.946873457511757,{"$f":"F6343*(1-Elteq!$F$9)","v":64.946873457511757},"8591735046347"]
["TECHNIK","M-1 PÁSKA  6 žlutá",null,"3476A026 kazeta se samolepicí páskou, šíře 6mm, návin 30m, barva žlutá","1ks",57.524373633796124,{"$f":"F6344*(1-Elteq!$F$9)","v":57.524373633796124},"8591735020491"]
["TECHNIK","M-1 PÁSKA  9 bílá",null,"3476A024 kazeta se samolepicí páskou, šíře 9mm, návin 30m, barva bílá","1ks",74.59612322834208,{"$f":"F6345*(1-Elteq!$F$9)","v":74.59612322834208},"8591735016340"]
["TECHNIK","M-1 PÁSKA  9 stříbr.",null,"3476A069 kazeta se samolepicí páskou, šíře 9mm, návin 27m, barva stříbrná","1ks",81.276373069686144,{"$f":"F6346*(1-Elteq!$F$9)","v":81.276373069686144},"8591735046354"]
["TECHNIK","M-1 PÁSKA  9 žlutá",null,"3476A027 kazeta se samolepicí páskou, šíře 9mm, návin 30m, barva žlutá","1ks",74.59612322834208,{"$f":"F6347*(1-Elteq!$F$9)","v":74.59612322834208},"8591735016357"]
["TECHNIK","M-1 PÁSKA 12 bílá",null,"3476A025 kazeta se samolepicí páskou, šíře 12mm, návin 30m, barva bílá","1ks",83.503123016800828,{"$f":"F6348*(1-Elteq!$F$9)","v":83.503123016800828},"8591735020507"]
["TECHNIK","M-1 PÁSKA 12 stříbr.",null,"3476A070 kazeta se samolepicí páskou, šíře 12mm, návin 27m, barva stříbrná","1ks",88.69887289340177,{"$f":"F6349*(1-Elteq!$F$9)","v":88.69887289340177},"8591735046361"]
["TECHNIK","M-1 PÁSKA 12 žlutá",null,"3476A028 kazeta se samolepicí páskou, šíře 12mm, návin 30m, barva žlutá","1ks",83.503123016800828,{"$f":"F6350*(1-Elteq!$F$9)","v":83.503123016800828},"8591735020514"]
["TECHNIK","M-1/CH TISK bílá",null,"Tisková páska s čipem pro tiskárny Canon M-1 Std. a M-1 Pro, návin 85m, barva bílá","1ks",27.83437433893361,{"$f":"F6351*(1-Elteq!$F$9)","v":27.83437433893361},"8591735042998"]
["TECHNIK","M-1/CH TISK bílá ID",null,"3607B001 tisková páska s čipem pro tiskárny Canon M-1 Std. a M-1 Pro, návin 85m, barva bílá ID","1ks",29.504436799269627,{"$f":"F6352*(1-Elteq!$F$9)","v":29.504436799269627},"8591735051372"]
["TECHNIK","M-1/CH TISK černá ID",null,"3604B001 tisková páska s čipem pro tiskárny Canon M-1 Std. a M-1 Pro, návin 100m, barva černá ID","1ks",29.504436799269627,{"$f":"F6353*(1-Elteq!$F$9)","v":29.504436799269627},"8591735048815"]
["TECHNIK","M-1/CH TISK černá MS",null,"3606B001 tisková páska s čipem pro tiskárny Canon M-1 Std. a M-1 Pro, návin 40m, barva černá MS","1ks",61.606748536839724,{"$f":"F6354*(1-Elteq!$F$9)","v":61.606748536839724},""]
["TECHNIK","S700E nůž",null,"Náhradní střihací nůž pro tiskárnu Biovin model S700E (KS-01)","1ks",16.329499612174384,{"$f":"F6355*(1-Elteq!$F$9)","v":16.329499612174384},"8591735050603"]
["TECHNIK","S700E PÁS 6 bílá",null,"Samolepicí páska pro tiskárnu S700E, návin 8m, šíře 6mm, barva bílá (LS-06W)","1ks",17.44287458573173,{"$f":"F6356*(1-Elteq!$F$9)","v":17.44287458573173},"8591735050610"]
["TECHNIK","S700E PÁS 6 stříbrná",null,"Samolepicí páska pro tiskárnu S700E, návin 8m, šíře 6mm, barva stříbrná (LS-06S)","1ks",17.44287458573173,{"$f":"F6357*(1-Elteq!$F$9)","v":17.44287458573173},"8591735050627"]
["TECHNIK","S700E PÁS 6 žlutá",null,"Samolepicí páska pro tiskárnu S700E, návin 8m, šíře 6mm, barva žlutá (LS-06Y)","1ks",17.44287458573173,{"$f":"F6358*(1-Elteq!$F$9)","v":17.44287458573173},"8591735050634"]
["TECHNIK","S700E PÁS 9 bílá",null,"Samolepicí páska pro tiskárnu S700E, návin 8m, šíře 9mm, barva bílá (LS-09W)","1ks",17.44287458573173,{"$f":"F6359*(1-Elteq!$F$9)","v":17.44287458573173},"8591735049997"]
["TECHNIK","S700E PÁS 9 stříbrná",null,"Samolepicí páska pro tiskárnu S700E, návin 8m, šíře 9mm, barva stříbrná (LS-09S)","1ks",17.44287458573173,{"$f":"F6360*(1-Elteq!$F$9)","v":17.44287458573173},"8591735050641"]
["TECHNIK","S700E PÁS 9 žlutá",null,"Samolepicí páska pro tiskárnu S700E, návin 8m, šíře 9mm, barva žlutá (LS-09Y)","1ks",17.44287458573173,{"$f":"F6361*(1-Elteq!$F$9)","v":17.44287458573173},"8591735050658"]
["TECHNIK","S700E PÁS12 bílá",null,"Samolepicí páska pro tiskárnu S700E, návin 8m, šíře 12mm, barva bílá (LS-12W)","1ks",17.44287458573173,{"$f":"F6362*(1-Elteq!$F$9)","v":17.44287458573173},"8591735050009"]
["TECHNIK","S700E PÁS12 stříbrná",null,"Samolepicí páska pro tiskárnu S700E, návin 8m, šíře 12mm, barva stříbrná (LS-12S)","1ks",17.44287458573173,{"$f":"F6363*(1-Elteq!$F$9)","v":17.44287458573173},"8591735050665"]
["TECHNIK","S700E PÁS12 žlutá",null,"Samolepicí páska pro tiskárnu S700E, návin 8m, šíře 12mm, barva žlutá (LS-12Y)","1ks",17.44287458573173,{"$f":"F6364*(1-Elteq!$F$9)","v":17.44287458573173},"8591735050672"]
["TECHNIK","S700E TISK černá",null,"Tisková páska pro tiskárnu Biovin model S700E, návin 80m, barva černá (RS-80B)","1ks",30.246686781641188,{"$f":"F6365*(1-Elteq!$F$9)","v":30.246686781641188},"8591735047443"]
["TECHNIK","TP80E nůž",null,"Náhradní střihací nůž pro tiskárnu TP80E (TP-HC12E)","1ks",17.81399957691751,{"$f":"F6366*(1-Elteq!$F$9)","v":17.81399957691751},""]
["TECHNIK","TP80E PÁS 6 bílá",null,"Samolepicí páska pro tiskárnu TP80E, návin 16m, šíře 6mm, barva bílá (TP-L06EW)","1ks",40.638186534843072,{"$f":"F6367*(1-Elteq!$F$9)","v":40.638186534843072},""]
["TECHNIK","TP80E PÁS 6 stříbrná",null,"Samolepicí páska pro tiskárnu TP80E, návin 16m, šíře 6mm, barva stříbrná (TP-L06ES)","1ks",40.638186534843072,{"$f":"F6368*(1-Elteq!$F$9)","v":40.638186534843072},""]
["TECHNIK","TP80E PÁS 6 žlutá",null,"Samolepicí páska pro tiskárnu TP80E, návin 16m, šíře 6mm, barva žlutá (TP-L06EY)","1ks",40.638186534843072,{"$f":"F6369*(1-Elteq!$F$9)","v":40.638186534843072},""]
["TECHNIK","TP80E PÁS 9 bílá",null,"Samolepicí páska pro tiskárnu TP80E, návin 16m, šíře 9mm, barva bílá (TP-L09EW)","1ks",40.638186534843072,{"$f":"F6370*(1-Elteq!$F$9)","v":40.638186534843072},""]
["TECHNIK","TP80E PÁS 9 stříbrná",null,"Samolepicí páska pro tiskárnu TP80E, návin 16m, šíře 9mm, barva stříbrná (TP-L09ES)","1ks",40.638186534843072,{"$f":"F6371*(1-Elteq!$F$9)","v":40.638186534843072},""]
["TECHNIK","TP80E PÁS 9 žlutá",null,"Samolepicí páska pro tiskárnu TP80E, návin 16m, šíře 9mm, barva žlutá (TP-L09EY)","1ks",40.638186534843072,{"$f":"F6372*(1-Elteq!$F$9)","v":40.638186534843072},""]
["TECHNIK","TP80E PÁS12 bílá",null,"Samolepicí páska pro tiskárnu TP80E, návin 16m, šíře 12mm, barva bílá (TP-L12EW)","1ks",40.638186534843072,{"$f":"F6373*(1-Elteq!$F$9)","v":40.638186534843072},""]
["TECHNIK","TP80E PÁS12 stříbrná",null,"Samolepicí páska pro tiskárnu TP80E, návin 16m, šíře 12mm, barva stříbrná (TP-L12ES)","1ks",40.638186534843072,{"$f":"F6374*(1-Elteq!$F$9)","v":40.638186534843072},""]
["TECHNIK","TP80E PÁS12 žlutá",null,"Samolepicí páska pro tiskárnu TP80E, návin 16m, šíře 12mm, barva žlutá (TP-L12EY)","1ks",40.638186534843072,{"$f":"F6375*(1-Elteq!$F$9)","v":40.638186534843072},""]
["TECHNIK","TP80E TISK černá",null,"Tisková páska pro tiskárnu TP80E, návin 100m, barva černá (TP-R100EB)","1ks",35.62799915383502,{"$f":"F6376*(1-Elteq!$F$9)","v":35.62799915383502},""]
["TECHNIK","XR- 6WE1",null,"Páska CASIO originální plastová samolepicí šíře 6mm, černá na bílém, návin 8m","1ks",17.44287458573173,{"$f":"F6377*(1-Elteq!$F$9)","v":17.44287458573173},"8591735043506"]
["TECHNIK","XR- 6WE1.C",null,"Páska CASIO kompatibilní plastová samolepicí šíře 6mm, černá na bílém, návin 8m","1ks",9.649249770830318,{"$f":"F6378*(1-Elteq!$F$9)","v":9.649249770830318},"8591735053741"]
["TECHNIK","XR- 6YW1.C",null,"Páska CASIO kompatibilní plastová samolepicí šíře 6mm, černá na žlutém, návin 8m","1ks",9.649249770830318,{"$f":"F6379*(1-Elteq!$F$9)","v":9.649249770830318},"8591735053758"]
["TECHNIK","XR- 9BU1",null,"Páska CASIO originální plastová samolepicí šíře 9mm, černá na modrém, návin 8m","1ks",19.484062037253526,{"$f":"F6380*(1-Elteq!$F$9)","v":19.484062037253526},""]
["TECHNIK","XR- 9GN1",null,"Páska CASIO originální plastová samolepicí šíře 9mm, černá na zeleném, návin 8m","1ks",19.484062037253526,{"$f":"F6381*(1-Elteq!$F$9)","v":19.484062037253526},""]
["TECHNIK","XR- 9RD1",null,"Páska CASIO originální plastová samolepicí šíře 9mm, černá na červeném, návin 8m","1ks",19.484062037253526,{"$f":"F6382*(1-Elteq!$F$9)","v":19.484062037253526},""]
["TECHNIK","XR- 9SR1",null,"Páska CASIO originální plastová samolepicí šíře 9mm, černá na stříbrném, návin 8m","1ks",19.484062037253526,{"$f":"F6383*(1-Elteq!$F$9)","v":19.484062037253526},""]
["TECHNIK","XR- 9WE1",null,"Páska CASIO originální plastová samolepicí šíře 9mm, černá na bílém, návin 8m","1ks",19.484062037253526,{"$f":"F6384*(1-Elteq!$F$9)","v":19.484062037253526},""]
["TECHNIK","XR- 9WE1.C",null,"Páska CASIO kompatibilní plastová samolepicí šíře 9mm, černá na bílém, návin 8m","1ks",9.649249770830318,{"$f":"F6385*(1-Elteq!$F$9)","v":9.649249770830318},"8591735053413"]
["TECHNIK","XR- 9X1",null,"Páska CASIO originální plastová samolepicí šíře 9mm, černá na průhledném, návin 8m","1ks",19.484062037253526,{"$f":"F6386*(1-Elteq!$F$9)","v":19.484062037253526},""]
["TECHNIK","XR- 9X1.C",null,"Páska CASIO kompatibilní plastová samolepicí šíře 9mm, černá na průhledném, návin 8m","1ks",9.649249770830318,{"$f":"F6387*(1-Elteq!$F$9)","v":9.649249770830318},"8591735053680"]
["TECHNIK","XR- 9YW1",null,"Páska CASIO originální plastová samolepicí šíře 9mm, černá na žlutém, návin 8m","1ks",19.484062037253526,{"$f":"F6388*(1-Elteq!$F$9)","v":19.484062037253526},""]
["TECHNIK","XR- 9YW1.C",null,"Páska CASIO kompatibilní plastová samolepicí šíře 9mm, černá na žlutém, návin 8m","1ks",9.649249770830318,{"$f":"F6389*(1-Elteq!$F$9)","v":9.649249770830318},"8591735054335"]
["TECHNIK","XR-12WE1",null,"Páska CASIO originální plastová samolepicí šíře 12mm, černá na bílém, návin 8m","1ks",21.154124497589542,{"$f":"F6390*(1-Elteq!$F$9)","v":21.154124497589542},""]
["TECHNIK","XR-12WE1.C",null,"Páska CASIO kompatibilní plastová samolepicí šíře 12mm, černá na bílém, návin 8m","1ks",10.948187239980554,{"$f":"F6391*(1-Elteq!$F$9)","v":10.948187239980554},"8591735053420"]
["TECHNIK","XR-12X1.C",null,"Páska CASIO kompatibilní plastová samolepicí šíře 12mm, černá na průhledném, návin 8m","1ks",10.948187239980554,{"$f":"F6392*(1-Elteq!$F$9)","v":10.948187239980554},"8591735053703"]
["TECHNIK","XR-12YW1",null,"Páska CASIO originální plastová samolepicí šíře 12mm, černá na žlutém, návin 8m","1ks",21.154124497589542,{"$f":"F6393*(1-Elteq!$F$9)","v":21.154124497589542},""]
["TECHNIK","XR-12YW1.C",null,"Páska CASIO kompatibilní plastová samolepicí šíře 12mm, černá na žlutém, návin 8m","1ks",10.948187239980554,{"$f":"F6394*(1-Elteq!$F$9)","v":10.948187239980554},"8591735054342"]
["TECHNIK","XR-18BU1",null,"Páska CASIO originální plastová samolepicí šíře 18mm, černá na modrém, návin 8m","1ks",23.751999435890014,{"$f":"F6395*(1-Elteq!$F$9)","v":23.751999435890014},""]
["TECHNIK","XR-18GN1",null,"Páska CASIO originální plastová samolepicí šíře 18mm, černá na zeleném, návin 8m","1ks",23.751999435890014,{"$f":"F6396*(1-Elteq!$F$9)","v":23.751999435890014},""]
["TECHNIK","XR-18RD1",null,"Páska CASIO originální plastová samolepicí šíře 18mm, černá na červeném, návin 8m","1ks",23.751999435890014,{"$f":"F6397*(1-Elteq!$F$9)","v":23.751999435890014},""]
["TECHNIK","XR-18SR1",null,"Páska CASIO originální plastová samolepicí šíře 18mm, černá na stříbrném, návin 8m","1ks",23.751999435890014,{"$f":"F6398*(1-Elteq!$F$9)","v":23.751999435890014},""]
["TECHNIK","XR-18WE1",null,"Páska CASIO originální plastová samolepicí šíře 18mm, černá na bílém, návin 8m","1ks",23.751999435890014,{"$f":"F6399*(1-Elteq!$F$9)","v":23.751999435890014},""]
["TECHNIK","XR-18WE1.C",null,"Páska CASIO kompatibilní plastová samolepicí šíře 18mm, černá na bílém, návin 8m","1ks",12.98937469150235,{"$f":"F6400*(1-Elteq!$F$9)","v":12.98937469150235},"8591735053697"]
["TECHNIK","XR-18X1",null,"Páska CASIO originální plastová samolepicí šíře 18mm, černá na průhledném, návin 8m","1ks",23.751999435890014,{"$f":"F6401*(1-Elteq!$F$9)","v":23.751999435890014},""]
["TECHNIK","XR-18YW1",null,"Páska CASIO originální plastová samolepicí šíře 18mm, černá na žlutém, návin 8m","1ks",23.751999435890014,{"$f":"F6402*(1-Elteq!$F$9)","v":23.751999435890014},""]
["TECHNIK","XR-18YW1.C",null,"Páska CASIO kompatibilní plastová samolepicí šíře 18mm, černá na žlutém, návin 8m","1ks",12.98937469150235,{"$f":"F6403*(1-Elteq!$F$9)","v":12.98937469150235},"8591735053710"]
["TECHNIK","XR-24WE1",null,"Páska CASIO originální plastová samolepicí šíře 24mm, černá na bílém, návin 8m","1ks",27.092124356562046,{"$f":"F6404*(1-Elteq!$F$9)","v":27.092124356562046},"8591735043513"]
["TECHNIK","XR-24WE1.C",null,"Páska CASIO kompatibilní plastová samolepicí šíře 24mm, černá na bílém, návin 8m","1ks",15.772812125395712,{"$f":"F6405*(1-Elteq!$F$9)","v":15.772812125395712},"8591735053727"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"XR-24YW1",null,"Páska CASIO originální plastová samolepicí šíře 24mm, černá na žlutém, návin 8m","1ks",27.092124356562046,{"$f":"F6406*(1-Elteq!$F$9)","v":27.092124356562046},"8591735043490"]
["TECHNIK","XR-24YW1.C",null,"Páska CASIO kompatibilní plastová samolepicí šíře 24mm, černá na žlutém, návin 8m","1ks",15.772812125395712,{"$f":"F6407*(1-Elteq!$F$9)","v":15.772812125395712},"8591735053734"]
["TECHNIK","S0718040",null,"16957 DYMO RHINO páska flexibilní nylonová šíře 12mm, černý tisk / bílý podklad, návin 3,5m","1ks",17.071749594545945,{"$f":"F6408*(1-Elteq!$F$9)","v":17.071749594545945},"5411313169578"]
["TECHNIK","S0718050",null,"16958 DYMO RHINO páska flexibilní nylonová šíře 19mm, černý tisk / bílý podklad, návin 3,5m","1ks",21.896374479961107,{"$f":"F6409*(1-Elteq!$F$9)","v":21.896374479961107},"5411313169585"]
["TECHNIK","S0718060",null,"16959 DYMO RHINO páska permanentní polyesterová šíře 12mm, černý tisk / bílý podklad, návin 3,5m","1ks",17.071749594545945,{"$f":"F6410*(1-Elteq!$F$9)","v":17.071749594545945},"5411313169592"]
["TECHNIK","S0718070",null,"16960 DYMO RHINO páska permanentní polyesterová šíře 19mm, černý tisk / bílý podklad, návin 3,5m","1ks",21.896374479961107,{"$f":"F6411*(1-Elteq!$F$9)","v":21.896374479961107},"5411313169608"]
["TECHNIK","S0718080",null,"18756,18490 DYMO RHINO páska flexibilní nylonová šíře 12mm, černý tisk / žlutý podklad, návin 3,5m","1ks",19.298499541660636,{"$f":"F6412*(1-Elteq!$F$9)","v":19.298499541660636},"0071701187567"]
["TECHNIK","S0718100",null,"18758,18488 DYMO RHINO páska flexibilní nylonová šíře 12mm, černý tisk / bílý podklad, návin 3,5m","1ks",19.298499541660636,{"$f":"F6413*(1-Elteq!$F$9)","v":19.298499541660636},"0071701187574"]
["TECHNIK","S0718120",null,"18759,18489 DYMO RHINO páska flexibilní nylonová šíře 19mm, černý tisk / bílý podklad, návin 3,5m","1ks",21.525249488775323,{"$f":"F6414*(1-Elteq!$F$9)","v":21.525249488775323},"0071701187581"]
["TECHNIK","S0718160",null,"18508 DYMO RHINO páska permanentní polyesterová šíře 9mm, černý tisk / průhledný podklad, návin 5,5m","1ks",16.329499612174384,{"$f":"F6415*(1-Elteq!$F$9)","v":16.329499612174384},""]
["TECHNIK","S0718170",null,"18760,18485 DYMO páska permanentní polyesterová šíře 9mm, černý tisk / metalický podklad, návin 5,5m","1ks",16.329499612174384,{"$f":"F6416*(1-Elteq!$F$9)","v":16.329499612174384},""]
["TECHNIK","S0718180",null,"18761,18486 DYMO páska permanentní polyesterová šíře 12mm, černý tisk / metalický podkl., návin 5,5m","1ks",17.44287458573173,{"$f":"F6417*(1-Elteq!$F$9)","v":17.44287458573173},""]
["TECHNIK","S0718200",null,"18762,18487 DYMO páska permanentní polyesterová šíře 19mm, černý tisk / metalický podkl., návin 5,5m","1ks",19.298499541660636,{"$f":"F6418*(1-Elteq!$F$9)","v":19.298499541660636},""]
["TECHNIK","S0718210",null,"18764,18483 DYMO páska permanentní polyesterová šíře 12mm, černý tisk / bílý podklad, návin 5,5m","1ks",17.44287458573173,{"$f":"F6419*(1-Elteq!$F$9)","v":17.44287458573173},"0071701187642"]
["TECHNIK","S0718220",null,"18765,18484 DYMO páska permanentní polyesterová šíře 19mm, černý tisk / bílý podklad, návin 5,5m","1ks",19.298499541660636,{"$f":"F6420*(1-Elteq!$F$9)","v":19.298499541660636},""]
["TECHNIK","S0718240",null,"18766,18482 DYMO páska permanentní polyesterová šíře 9mm, černý tisk / bílý podklad, návin  5,5m","1ks",16.329499612174384,{"$f":"F6421*(1-Elteq!$F$9)","v":16.329499612174384},""]
["TECHNIK","S0718260",null,"18051 DYMO plochá smršťovací bužírka šíře 6mm pro průměry 1,18-2,33mm, černý tisk na bílém (1,5m)","1ks",27.463249347747826,{"$f":"F6422*(1-Elteq!$F$9)","v":27.463249347747826},"0071701180513"]
["TECHNIK","S0718270",null,"18052 DYMO plochá smršťovací bužírka šíře 6mm pro průměry 1,18-2,33mm, černý tisk na žlutém (1,5m)","1ks",27.463249347747826,{"$f":"F6423*(1-Elteq!$F$9)","v":27.463249347747826},"0071701180520"]
["TECHNIK","S0718280",null,"18053 DYMO plochá smršťovací bužírka šíře 9mm pro průměry 1,73-3,73mm, černý tisk na bílém (1,5m)","1ks",28.576624321305172,{"$f":"F6424*(1-Elteq!$F$9)","v":28.576624321305172},"0071701180537"]
["TECHNIK","S0718280.C",null,"18053 DYMO kompatibilní smršťovací bužírka 9mm pro průměry 1,73-3,73mm, černý tisk na bílém (1,5m)","1ks",21.525249488775323,{"$f":"F6425*(1-Elteq!$F$9)","v":21.525249488775323},""]
["TECHNIK","S0718290",null,"18054 DYMO plochá smršťovací bužírka šíře 9mm pro průměry 1,73-3,73mm, černý tisk na žlutém (1,5m)","1ks",28.576624321305172,{"$f":"F6426*(1-Elteq!$F$9)","v":28.576624321305172},"0071701180544"]
["TECHNIK","S0718290.C",null,"18054 DYMO kompatibilní smršťovací bužírka 9mm pro průměry 1,73-3,73mm, černý tisk na žlutém (1,5m)","1ks",21.525249488775323,{"$f":"F6427*(1-Elteq!$F$9)","v":21.525249488775323},""]
["TECHNIK","S0718300",null,"18055 DYMO plochá smršťovací bužírka šíře 12mm pro průměry 2,97-5,13mm, černý tisk na bílém (1,5m)","1ks",30.617811772826972,{"$f":"F6428*(1-Elteq!$F$9)","v":30.617811772826972},"0071701180551"]
["TECHNIK","S0718300.C",null,"18055 DYMO kompatibilní smršťovací bužírka 12mm pro průměry 2,97-5,13mm, černý tisk na bílém (1,5m)","1ks",22.638624462332668,{"$f":"F6429*(1-Elteq!$F$9)","v":22.638624462332668},""]
["TECHNIK","S0718310",null,"18056 DYMO plochá smršťovací bužírka šíře 12mm pro průměry 2,97-5,13mm, černý tisk na žlutém (1,5m)","1ks",30.617811772826972,{"$f":"F6430*(1-Elteq!$F$9)","v":30.617811772826972},"0071701180568"]
["TECHNIK","S0718310.C",null,"18056 DYMO kompatibilní smršťovací bužírka 12mm pro průměry 2,97-5,13mm, černý tisk na žlutém (1,5m)","1ks",22.638624462332668,{"$f":"F6431*(1-Elteq!$F$9)","v":22.638624462332668},""]
["TECHNIK","S0718330",null,"18057 DYMO plochá smršťovací bužírka šíře 19mm pro průměry 4,64-8,70mm, černý tisk na bílém (1,5m)","1ks",33.215686711127439,{"$f":"F6432*(1-Elteq!$F$9)","v":33.215686711127439},""]
["TECHNIK","S0718340",null,"18058 DYMO plochá smršťovací bužírka šíře 19mm pro průměry 4,64-8,70mm, černý tisk na žlutém (1,5m)","1ks",33.215686711127439,{"$f":"F6433*(1-Elteq!$F$9)","v":33.215686711127439},""]
["TECHNIK","S0718440",null,"18431 DYMO RHINO páska permanentní vinylová šíře 9mm, černý tisk / žlutý podklad, návin 5,5m","1ks",16.329499612174384,{"$f":"F6434*(1-Elteq!$F$9)","v":16.329499612174384},""]
["TECHNIK","S0718450",null,"18432 DYMO páska vinylová šíře 12mm, černý tisk / žlutý podklad, návin 5,5m","1ks",17.44287458573173,{"$f":"F6435*(1-Elteq!$F$9)","v":17.44287458573173},""]
["TECHNIK","S0718450.C",null,"18432 DYMO kompatibilní páska vinylová šíře 12mm, černý tisk / žlutý podklad, návin 5,5m","1ks",14.844999647431258,{"$f":"F6436*(1-Elteq!$F$9)","v":14.844999647431258},""]
["TECHNIK","S0718470",null,"18433 DYMO páska vinylová šíře 19mm, černý tisk / žlutý podklad, návin 5,5m","1ks",19.298499541660636,{"$f":"F6437*(1-Elteq!$F$9)","v":19.298499541660636},""]
["TECHNIK","S0718500",null,"18436 DYMO páska vinylová šíře 19mm, černý tisk / oranžový podklad, návin 5,5m","1ks",19.298499541660636,{"$f":"F6438*(1-Elteq!$F$9)","v":19.298499541660636},""]
["TECHNIK","S0718510",null,"18437 DYMO páska vinylová šíře 9mm, černý tisk / červený podklad, návin 5,5m","1ks",16.329499612174384,{"$f":"F6439*(1-Elteq!$F$9)","v":16.329499612174384},""]
["TECHNIK","S0718520",null,"18438 DYMO páska vinylová šíře 12mm, černý tisk / červený podklad, návin 5,5m","1ks",17.44287458573173,{"$f":"F6440*(1-Elteq!$F$9)","v":17.44287458573173},""]
["TECHNIK","S0718530",null,"18439 DYMO páska vinylová šíře 19mm, černý tisk / červený podklad, návin 5,5m","1ks",19.298499541660636,{"$f":"F6441*(1-Elteq!$F$9)","v":19.298499541660636},""]
["TECHNIK","S0718580",null,"18443 DYMO páska vinylová šíře 9mm, černý tisk / bílý podklad, návin 5,5m","1ks",16.329499612174384,{"$f":"F6442*(1-Elteq!$F$9)","v":16.329499612174384},""]
["TECHNIK","S0718580.C",null,"18443 DYMO kompatibilní páska vinylová šíře 9mm, černý tisk / bílý podklad, návin 5,5m","1ks",14.659437151838368,{"$f":"F6443*(1-Elteq!$F$9)","v":14.659437151838368},""]
["TECHNIK","S0718600",null,"18444 DYMO páska vinylová šíře 12mm, černý tisk / bílý podklad, návin 5,5m","1ks",17.44287458573173,{"$f":"F6444*(1-Elteq!$F$9)","v":17.44287458573173},""]
["TECHNIK","S0718620",null,"18445 DYMO páska vinylová šíře 19mm, černý tisk / bílý podklad, návin 5,5m","1ks",19.298499541660636,{"$f":"F6445*(1-Elteq!$F$9)","v":19.298499541660636},""]
["TECHNIK","S0718860",null,"18770 DYMO páska nažehlovací šíře 12mm, černý tisk / bílý podklad, návin 2m","1ks",7.7936248149014107,{"$f":"F6446*(1-Elteq!$F$9)","v":7.7936248149014107},"5411313187701"]
["TECHNIK","S0720500",null,"45010 DYMO páska plastová 12mm, černý tisk / průhledný podklad, návin 7m","1ks",17.81399957691751,{"$f":"F6447*(1-Elteq!$F$9)","v":17.81399957691751},"5411313450102"]
["TECHNIK","S0720510",null,"45011 DYMO páska plastová 12mm, modrý tisk / průhledný podklad, návin 7m","1ks",17.81399957691751,{"$f":"F6448*(1-Elteq!$F$9)","v":17.81399957691751},"5411313450119"]
["TECHNIK","S0720520",null,"45012 DYMO páska plastová 12mm, červený tisk / průhledný podklad, návin 7m","1ks",17.81399957691751,{"$f":"F6449*(1-Elteq!$F$9)","v":17.81399957691751},"5411313450126"]
["TECHNIK","S0720530",null,"45013 DYMO páska plastová 12mm, černý tisk / bílý podklad, návin 7m","1ks",17.81399957691751,{"$f":"F6450*(1-Elteq!$F$9)","v":17.81399957691751},"5411313450133"]
["TECHNIK","S0720530.C",null,"45013 DYMO kompatibilní páska plastová 12mm, černý tisk / bílý podklad, návin 7m","1ks",11.133749735573444,{"$f":"F6451*(1-Elteq!$F$9)","v":11.133749735573444},"8591735053376"]
["TECHNIK","S0720540",null,"45014 DYMO páska plastová 12mm, modrý tisk / bílý podklad, návin 7m","1ks",17.81399957691751,{"$f":"F6452*(1-Elteq!$F$9)","v":17.81399957691751},"5411313450140"]
["TECHNIK","S0720550",null,"45015 DYMO páska plastová 12mm, červený tisk / bílý podklad, návin 7m","1ks",17.81399957691751,{"$f":"F6453*(1-Elteq!$F$9)","v":17.81399957691751},"5411313450157"]
["TECHNIK","S0720560",null,"45016 DYMO páska plastová 12mm, černý tisk / modrý podklad, návin 7m","1ks",17.81399957691751,{"$f":"F6454*(1-Elteq!$F$9)","v":17.81399957691751},"5411313450164"]
["TECHNIK","S0720570",null,"45017 DYMO páska plastová 12mm, černý tisk / červený podklad, návin 7m","1ks",17.81399957691751,{"$f":"F6455*(1-Elteq!$F$9)","v":17.81399957691751},"5411313450171"]
["TECHNIK","S0720580",null,"45018 DYMO páska plastová 12mm, černý tisk / žlutý podklad, návin 7m","1ks",17.81399957691751,{"$f":"F6456*(1-Elteq!$F$9)","v":17.81399957691751},"5411313450188"]
["TECHNIK","S0720580.C",null,"45018 DYMO kompatibilní páska plastová 12mm, černý tisk / žlutý podklad, návin 7m","1ks",11.133749735573444,{"$f":"F6457*(1-Elteq!$F$9)","v":11.133749735573444},"8591735053383"]
["TECHNIK","S0720590",null,"45019 DYMO páska plastová 12mm, černý tisk / zelený podklad, návin 7m","1ks",17.81399957691751,{"$f":"F6458*(1-Elteq!$F$9)","v":17.81399957691751},"5411313450195"]
["TECHNIK","S0720600",null,"45020 DYMO páska plastová 12mm, bílý tisk / průhledný podklad, návin 7m","1ks",17.81399957691751,{"$f":"F6459*(1-Elteq!$F$9)","v":17.81399957691751},"5411313450201"]
["TECHNIK","S0720610",null,"45021 DYMO páska plastová 12mm, bílý tisk / černý podklad, návin 7m","1ks",17.81399957691751,{"$f":"F6460*(1-Elteq!$F$9)","v":17.81399957691751},"5411313450218"]
["TECHNIK","S0720670",null,"40910 DYMO páska plastová 9mm, černý tisk / průhledný podklad, návin 7m","1ks",16.700624603360165,{"$f":"F6461*(1-Elteq!$F$9)","v":16.700624603360165},"5411313409100"]
["TECHNIK","S0720670.C",null,"40910 DYMO kompatibilní páska plastová 9mm, černý tisk / průhledný podklad, návin 7m","1ks",11.133749735573444,{"$f":"F6462*(1-Elteq!$F$9)","v":11.133749735573444},"8591735053345"]
["TECHNIK","S0720680",null,"40913 DYMO páska plastová 9mm, černý tisk / bílý podklad, návin 7m","1ks",16.700624603360165,{"$f":"F6463*(1-Elteq!$F$9)","v":16.700624603360165},"5411313409131"]
["TECHNIK","S0720680.C",null,"40913 DYMO kompatibilní páska plastová 9mm, černý tisk / bílý podklad, návin 7m","1ks",11.133749735573444,{"$f":"F6464*(1-Elteq!$F$9)","v":11.133749735573444},"8591735053352"]
["TECHNIK","S0720690",null,"40914 DYMO páska plastová 9mm, modrý tisk / bílý podklad, návin 7m","1ks",16.700624603360165,{"$f":"F6465*(1-Elteq!$F$9)","v":16.700624603360165},"5411313409148"]
["TECHNIK","S0720700",null,"40915 DYMO páska plastová 9mm, červený tisk / bílý podklad, návin 7m","1ks",16.700624603360165,{"$f":"F6466*(1-Elteq!$F$9)","v":16.700624603360165},"5411313409155"]
["TECHNIK","S0720710",null,"40916 DYMO páska plastová 9mm, černý tisk / modrý podklad, návin 7m","1ks",16.700624603360165,{"$f":"F6467*(1-Elteq!$F$9)","v":16.700624603360165},"5411313409162"]
["TECHNIK","S0720720",null,"40917 DYMO páska plastová 9mm, černý tisk / červený podklad, návin 7m","1ks",16.700624603360165,{"$f":"F6468*(1-Elteq!$F$9)","v":16.700624603360165},"5411313409179"]
["TECHNIK","S0720730",null,"40918 DYMO páska plastová 9mm, černý tisk / žlutý podklad, návin 7m","1ks",16.700624603360165,{"$f":"F6469*(1-Elteq!$F$9)","v":16.700624603360165},"5411313409186"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"S0720730.C",null,"40918 DYMO kompatibilní páska plastová 9mm, černý tisk / žlutý podklad, návin 7m","1ks",11.133749735573444,{"$f":"F6470*(1-Elteq!$F$9)","v":11.133749735573444},"8591735053369"]
["TECHNIK","S0720740",null,"40919 DYMO páska plastová 9mm, černý tisk / zelený podklad, návin 7m","1ks",16.700624603360165,{"$f":"F6471*(1-Elteq!$F$9)","v":16.700624603360165},"5411313409193"]
["TECHNIK","S0720770",null,"43610 DYMO páska plastová 6mm, černý tisk / průhledný podklad, návin 7m","1ks",15.772812125395712,{"$f":"F6472*(1-Elteq!$F$9)","v":15.772812125395712},"5411313436106"]
["TECHNIK","S0720780",null,"43613 DYMO páska plastová 6mm, černý tisk / bílý podklad, návin 7m","1ks",15.772812125395712,{"$f":"F6473*(1-Elteq!$F$9)","v":15.772812125395712},"5411313436137"]
["TECHNIK","S0720790",null,"43618 DYMO páska plastová 6mm, černý tisk / žlutý podklad, návin 7m","1ks",15.772812125395712,{"$f":"F6474*(1-Elteq!$F$9)","v":15.772812125395712},"5411313436380"]
["TECHNIK","S0720820",null,"45800 DYMO páska plastová 19mm, černý tisk / průhledný podklad, návin 7m","1ks",22.638624462332668,{"$f":"F6475*(1-Elteq!$F$9)","v":22.638624462332668},"5411313452106"]
["TECHNIK","S0720830",null,"45803 DYMO páska plastová 19mm, černý tisk / bílý podklad, návin 7m","1ks",22.638624462332668,{"$f":"F6476*(1-Elteq!$F$9)","v":22.638624462332668},"5411313452137"]
["TECHNIK","S0720830.C",null,"45803 DYMO kompatibilní páska plastová 19mm, černý tisk / bílý podklad, návin 7m","1ks",13.174937187095242,{"$f":"F6477*(1-Elteq!$F$9)","v":13.174937187095242},"8591735053390"]
["TECHNIK","S0720840",null,"45804 DYMO páska plastová 19mm, modrý tisk / bílý podklad, návin 7m","1ks",22.638624462332668,{"$f":"F6478*(1-Elteq!$F$9)","v":22.638624462332668},"5411313452144"]
["TECHNIK","S0720850",null,"45805 DYMO páska plastová 19mm, červený tisk / bílý podklad, návin 7m","1ks",22.638624462332668,{"$f":"F6479*(1-Elteq!$F$9)","v":22.638624462332668},"5411313452151"]
["TECHNIK","S0720860",null,"45806 DYMO páska plastová 19mm, černý tisk / modrý podklad, návin 7m","1ks",22.638624462332668,{"$f":"F6480*(1-Elteq!$F$9)","v":22.638624462332668},"5411313452168"]
["TECHNIK","S0720870",null,"45807 DYMO páska plastová 19mm, černý tisk / červený podklad, návin 7m","1ks",22.638624462332668,{"$f":"F6481*(1-Elteq!$F$9)","v":22.638624462332668},"5411313452175"]
["TECHNIK","S0720880",null,"45808 DYMO páska plastová 19mm, černý tisk / žlutý podklad, návin 7m","1ks",22.638624462332668,{"$f":"F6482*(1-Elteq!$F$9)","v":22.638624462332668},"5411313452182"]
["TECHNIK","S0720880.C",null,"45808 DYMO kompatibilní páska plastová 19mm, černý tisk / žlutý podklad, návin 7m","1ks",13.174937187095242,{"$f":"F6483*(1-Elteq!$F$9)","v":13.174937187095242},"8591735053406"]
["TECHNIK","S0720890",null,"45809 DYMO páska plastová 19mm, černý tisk / zelený podklad, návin 7m","1ks",22.638624462332668,{"$f":"F6484*(1-Elteq!$F$9)","v":22.638624462332668},"5411313452199"]
["TECHNIK","S0720900",null,"45810 DYMO páska plastová 19mm, bílý tisk / průhledný podklad, návin 7m","1ks",22.638624462332668,{"$f":"F6485*(1-Elteq!$F$9)","v":22.638624462332668},"5411313452205"]
["TECHNIK","S0720910",null,"45811 DYMO páska plastová 19mm, bílý tisk / černý podklad, návin 7m","1ks",22.638624462332668,{"$f":"F6486*(1-Elteq!$F$9)","v":22.638624462332668},"5411313452212"]
["TECHNIK","S0720920",null,"53710 DYMO páska plastová 24mm, černý tisk / průhledný podklad, návin 7m","1ks",25.79318688741181,{"$f":"F6487*(1-Elteq!$F$9)","v":25.79318688741181},"5411313537100"]
["TECHNIK","S0720930",null,"53713 DYMO páska plastová 24mm, černý tisk / bílý podklad, návin 7m","1ks",25.79318688741181,{"$f":"F6488*(1-Elteq!$F$9)","v":25.79318688741181},"5411313537131"]
["TECHNIK","S0720930.C",null,"53713 DYMO kompatibilní páska plastová 24mm, černý tisk / bílý podklad, návin 7m","1ks",15.216124638617039,{"$f":"F6489*(1-Elteq!$F$9)","v":15.216124638617039},"8591735053529"]
["TECHNIK","S0720940",null,"53714 DYMO páska plastová 24mm, modrý tisk / bílý podklad, návin 7m","1ks",25.79318688741181,{"$f":"F6490*(1-Elteq!$F$9)","v":25.79318688741181},"5411313537148"]
["TECHNIK","S0720950",null,"53715 DYMO páska plastová 24mm, červený tisk / bílý podklad, návin 7m","1ks",25.79318688741181,{"$f":"F6491*(1-Elteq!$F$9)","v":25.79318688741181},"5411313537155"]
["TECHNIK","S0720960",null,"53716 DYMO páska plastová 24mm, černý tisk / modrý podklad, návin 7m","1ks",25.79318688741181,{"$f":"F6492*(1-Elteq!$F$9)","v":25.79318688741181},"5411313537162"]
["TECHNIK","S0720970",null,"53717 DYMO páska plastová 24mm, černý tisk / červený podklad, návin 7m","1ks",25.79318688741181,{"$f":"F6493*(1-Elteq!$F$9)","v":25.79318688741181},"5411313537179"]
["TECHNIK","S0720980",null,"53718 DYMO páska plastová 24mm, černý tisk / žlutý podklad, návin 7m","1ks",25.79318688741181,{"$f":"F6494*(1-Elteq!$F$9)","v":25.79318688741181},"5411313537186"]
["TECHNIK","S0720980.C",null,"53718 DYMO kompatibilní páska plastová 24mm, černý tisk / žlutý podklad, návin 7m","1ks",15.216124638617039,{"$f":"F6495*(1-Elteq!$F$9)","v":15.216124638617039},"8591735053536"]
["TECHNIK","S0720990",null,"53719 DYMO páska plastová 24mm, černý tisk / zelený podklad, návin 7m","1ks",25.79318688741181,{"$f":"F6496*(1-Elteq!$F$9)","v":25.79318688741181},"5411313537193"]
["TECHNIK","S0721000",null,"53720 DYMO páska plastová 24mm, bílý tisk / průhledný podklad, návin 7m","1ks",25.79318688741181,{"$f":"F6497*(1-Elteq!$F$9)","v":25.79318688741181},"5411313537209"]
["TECHNIK","S0721010",null,"53721 DYMO páska plastová 24mm, bílý tisk / černý podklad, návin 7m","1ks",25.79318688741181,{"$f":"F6498*(1-Elteq!$F$9)","v":25.79318688741181},"5411313537216"]
["TECHNIK","S0773830",null,"1734523 DYMO RHINO páska polyesterová šíře 24mm samolepicí, černý tisk / bílý podklad, návin 5,5m","1ks",22.638624462332668,{"$f":"F6499*(1-Elteq!$F$9)","v":22.638624462332668},""]
["TECHNIK","S0773860",null,"1734821 DYMO RHINO páska obmotávací samolaminovací šíře 24mm, černý tisk / bílý podklad, návin 5,5m","1ks",22.638624462332668,{"$f":"F6500*(1-Elteq!$F$9)","v":22.638624462332668},""]
["TECHNIK","S1805416",null,"1805416 DYMO páska vinylová šíře 12mm, bílý tisk / červený podklad, návin 5,5m","1ks",17.44287458573173,{"$f":"F6501*(1-Elteq!$F$9)","v":17.44287458573173},""]
["TECHNIK","S1805417",null,"1805417 DYMO páska vinylová šíře 19mm, bílý tisk / modrý podklad, návin 5,5m","1ks",19.298499541660636,{"$f":"F6502*(1-Elteq!$F$9)","v":19.298499541660636},""]
["TECHNIK","S1805420",null,"1805420 DYMO páska vinylová šíře 19mm, bílý tisk / zelený podklad, návin 5,5m","1ks",19.298499541660636,{"$f":"F6503*(1-Elteq!$F$9)","v":19.298499541660636},""]
["TECHNIK","S1805422",null,"1805422 DYMO páska vinylová šíře 19mm, bílý tisk / červený podklad, návin 5,5m","1ks",19.298499541660636,{"$f":"F6504*(1-Elteq!$F$9)","v":19.298499541660636},""]
["TECHNIK","S1805440",null,"1805440 DYMO páska polyesterová šíře 6mm, černý tisk / průhledný podklad, návin 5,5m","1ks",15.587249629802821,{"$f":"F6505*(1-Elteq!$F$9)","v":15.587249629802821},""]
["TECHNIK","S1805443",null,"1805443 DYMO plochá smršťovací bužírka šíře 24mm pro průměry 6,5-14mm, černý tisk na bílém (1,5m)","1ks",37.29806161417104,{"$f":"F6506*(1-Elteq!$F$9)","v":37.29806161417104},""]
["TECHNIK","S1805444",null,"1805444 DYMO plochá smršťovací bužírka šíře 24mm pro průměry 6,5-14mm, černý tisk na žlutém (1,5m)","1ks",37.29806161417104,{"$f":"F6507*(1-Elteq!$F$9)","v":37.29806161417104},""]
["TECHNIK","S0721030",null,"60611 DYMO podkladová páska 6mm x 10m, bílá","1ks",12.247124709130787,{"$f":"F6508*(1-Elteq!$F$9)","v":12.247124709130787},"5411313606110"]
["TECHNIK","S0721090",null,"61211 DYMO podkladová páska 12mm x 10m, bílá","1ks",13.546062178281023,{"$f":"F6509*(1-Elteq!$F$9)","v":13.546062178281023},"5411313612111"]
["TECHNIK","S0721120",null,"61214 DYMO podkladová páska 12mm x 10m, žlutá","1ks",13.546062178281023,{"$f":"F6510*(1-Elteq!$F$9)","v":13.546062178281023},"5411313619141"]
["TECHNIK","S0721140",null,"61910 DYMO podkladová páska 19mm x 10m, průhledná","1ks",16.886187098953055,{"$f":"F6511*(1-Elteq!$F$9)","v":16.886187098953055},"5411313619103"]
["TECHNIK","S0721150",null,"61911 DYMO podkladová páska 19mm x 10m, bílá","1ks",16.886187098953055,{"$f":"F6512*(1-Elteq!$F$9)","v":16.886187098953055},"5411313619516"]
["TECHNIK","S0721180",null,"61914 DYMO podkladová páska 19mm x 10m, žlutá","1ks",16.886187098953055,{"$f":"F6513*(1-Elteq!$F$9)","v":16.886187098953055},"5411313619547"]
["TECHNIK","S0721210",null,"69241 DYMO podkladová páska 24mm x 10m, bílá","1ks",23.380874444704233,{"$f":"F6514*(1-Elteq!$F$9)","v":23.380874444704233},"5411313692410"]
["TECHNIK","S0721250",null,"69321 DYMO podkladová páska 32mm x 10m, bílá","1ks",28.019936834526501,{"$f":"F6515*(1-Elteq!$F$9)","v":28.019936834526501},"5411313693219"]
["TECHNIK","S0721280",null,"69324 DYMO podkladová páska 32mm x 10m, žlutá","1ks",28.019936834526501,{"$f":"F6516*(1-Elteq!$F$9)","v":28.019936834526501},"5411313693240"]
["TECHNIK","S0721300",null,"60601 DYMO tisková páska 19mm x 50m, černá","1ks",19.298499541660636,{"$f":"F6517*(1-Elteq!$F$9)","v":19.298499541660636},"5411313606011"]
["TECHNIK","S0721330",null,"63201 DYMO tisková páska 32mm x 50m, černá","1ks",24.865374409447359,{"$f":"F6518*(1-Elteq!$F$9)","v":24.865374409447359},"5411313632010"]
["TECHNIK","S0721500",null,"59421 DYMO páska papírová šíře 12mm / návin 4m, pro LetraTag, barva bílá","1ks",6.6802498413440663,{"$f":"F6519*(1-Elteq!$F$9)","v":6.6802498413440663},"5411313594219"]
["TECHNIK","S0721500.C",null,"59421 DYMO kompatibilní páska papírová šíře 12mm / návin 4m, pro LetraTag, barva bílá","1ks",6.3091248501582848,{"$f":"F6520*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735053543"]
["TECHNIK","S0721540",null,"12268 DYMO páska plastová šíře 12mm / návin 4m, pro LetraTag, průhledná","1ks",7.7936248149014107,{"$f":"F6521*(1-Elteq!$F$9)","v":7.7936248149014107},"5411313122689"]
["TECHNIK","S0721560",null,"59422 DYMO páska plastová šíře 12mm / návin 4m, pro LetraTag, barva bílá","1ks",7.7936248149014107,{"$f":"F6522*(1-Elteq!$F$9)","v":7.7936248149014107},"5411313594226"]
["TECHNIK","S0721560.C",null,"59422 DYMO kompatibilní páska plastová šíře 12mm / návin 4m, pro LetraTag, barva bílá","1ks",6.3091248501582848,{"$f":"F6523*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735053550"]
["TECHNIK","S0721570",null,"59423 DYMO páska plastová šíře 12mm / návin 4m, pro LetraTag, barva žlutá","1ks",7.7936248149014107,{"$f":"F6524*(1-Elteq!$F$9)","v":7.7936248149014107},"5411313594233"]
["TECHNIK","S0721570.C",null,"59423 DYMO kompatibilní páska plastová šíře 12mm / návin 4m, pro LetraTag, barva žlutá","1ks",6.3091248501582848,{"$f":"F6525*(1-Elteq!$F$9)","v":6.3091248501582848},"8591735053567"]
["TECHNIK","S0721580",null,"59424 DYMO páska plastová šíře 12mm / návin 4m, pro LetraTag, barva červená","1ks",7.7936248149014107,{"$f":"F6526*(1-Elteq!$F$9)","v":7.7936248149014107},"5411313594240"]
["TECHNIK","S0721590",null,"59425 DYMO páska plastová šíře 12mm / návin 4m, pro LetraTag, barva zelená","1ks",7.7936248149014107,{"$f":"F6527*(1-Elteq!$F$9)","v":7.7936248149014107},"5411313594257"]
["TECHNIK","S0721600",null,"59426 DYMO páska plastová šíře 12mm / návin 4m, pro LetraTag, barva modrá","1ks",7.7936248149014107,{"$f":"F6528*(1-Elteq!$F$9)","v":7.7936248149014107},"5411313594264"]
["TECHNIK","S0721710",null,"59429 DYMO páska plastová šíře 12mm / návin 4m, pro LetraTag, metalická stříbrná","1ks",8.5358747972729727,{"$f":"F6529*(1-Elteq!$F$9)","v":8.5358747972729727},"5411313594295"]
["TECHNIK","S0721720",null,"59430 DYMO páska plastová šíře 12mm / návin 4m, pro LetraTag, metalická zelená","1ks",8.5358747972729727,{"$f":"F6530*(1-Elteq!$F$9)","v":8.5358747972729727},"5411313594301"]
["TECHNIK","S0720160",null,"31000 DYMO RHINO páska hliníková bez lepidla pro přístroj M1011, šíře 12mm, návin 4,8m","1ks",7.0513748325298478,{"$f":"F6531*(1-Elteq!$F$9)","v":7.0513748325298478},"5411313310000"]
["TECHNIK","S0720170",null,"32500 DYMO RHINO páska nerezová bez lepidla pro přístroj M1011, šíře 12mm, návin 6,4m","1ks",10.020374762016099,{"$f":"F6532*(1-Elteq!$F$9)","v":10.020374762016099},"5411313325004"]
["TECHNIK","S0720180",null,"35800 DYMO RHINO páska hliníková s lepidlem pro přístroj M1011, šíře 12mm, návin 3,65m","1ks",10.205937257608991,{"$f":"F6533*(1-Elteq!$F$9)","v":10.205937257608991},"5411313358002"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"S0720290",null,"527206 DYMO plastová samolepicí páska typ 3D šíře 6mm, návin 3m, modrá","1ks",2.5607624391818922,{"$f":"F6534*(1-Elteq!$F$9)","v":2.5607624391818922},""]
["TECHNIK","S0720300",null,"527209 DYMO plastová samolepicí páska typ 3D šíře 6mm, návin 3m, černá","1ks",2.5607624391818922,{"$f":"F6535*(1-Elteq!$F$9)","v":2.5607624391818922},""]
["TECHNIK","S0810090",null,"DYMO nylonová bílá páska šíře 19mm samolepicí pro RHINO 101, návin 3,5m","1ks",10.948187239980554,{"$f":"F6536*(1-Elteq!$F$9)","v":10.948187239980554},"3501170810095"]
["TECHNIK","S0810130",null,"DYMO vinylová páska se štítky 19x38mm / značící pole 19x12mm pro RHINO 101 (140 štítků)","1ks",10.948187239980554,{"$f":"F6537*(1-Elteq!$F$9)","v":10.948187239980554},"3501170810132"]
["TECHNIK","S0810170",null,"DYMO vinylová páska se štítky 19x50mm / značící pole 19x16mm pro RHINO 101 (100 štítků)","1ks",10.948187239980554,{"$f":"F6538*(1-Elteq!$F$9)","v":10.948187239980554},"3501170810170"]
["TECHNIK","S0810210",null,"DYMO vinylová páska se štítky 19x76mm / značící pole 19x19mm pro RHINO 101 (75 štítků)","1ks",10.948187239980554,{"$f":"F6539*(1-Elteq!$F$9)","v":10.948187239980554},"3501170810217"]
["TECHNIK","S0810330",null,"DYMO vinylová páska se štítky 19x25mm / značící pole 19x 8mm pro RHINO 101 (200 štítků)","1ks",10.948187239980554,{"$f":"F6540*(1-Elteq!$F$9)","v":10.948187239980554},"3501170810330"]
["TECHNIK","S0847730",null,"DYMO plastová páska typ 3D šíře 9mm samolepicí, barva černá, návin 3m, blistr","3ks",5.9379998589725034,{"$f":"F6541*(1-Elteq!$F$9)","v":5.9379998589725034},"3501170847732"]
["TECHNIK","S0847740",null,"DYMO plastová páska typ 3D šíře 9mm samolepicí, barva modrá, návin 3m, blistr","3ks",5.9379998589725034,{"$f":"F6542*(1-Elteq!$F$9)","v":5.9379998589725034},"3501170847749"]
["TECHNIK","S0847750",null,"DYMO plastová páska typ 3D šíře 9mm samolepicí, mix černá / modrá / červená, návin 3m, blistr","3ks",5.9379998589725034,{"$f":"F6543*(1-Elteq!$F$9)","v":5.9379998589725034},"3501170847756"]
["TECHNIK","S0898130",null,"524709 (12745) páska typ 3D šíře 9mm samolepicí, návin 3m, černá (dříve S0720270)-blistr 2ks","1ks",2.6720999365376263,{"$f":"F6544*(1-Elteq!$F$9)","v":2.6720999365376263},"3501170898130"]
["TECHNIK","S0898140",null,"524706 (12744) páska typ 3D šíře 9mm samolepicí, návin 3m, modrá (dříve S0720250)-blistr 2ks","1ks",2.6720999365376263,{"$f":"F6545*(1-Elteq!$F$9)","v":2.6720999365376263},"3501170898147"]
["TECHNIK","S0898150",null,"524702 (12742) páska typ 3D šíře 9mm samolepicí, návin 3m, červená (dříve S0720220)-blistr 2ks","1ks",2.6720999365376263,{"$f":"F6546*(1-Elteq!$F$9)","v":2.6720999365376263},"3501170898154"]
["TECHNIK","S0898160",null,"524705 (12743) páska typ 3D šíře 9mm samolepicí, návin 3m, zelená (dříve S0720240)-blistr 2ks","1ks",2.6720999365376263,{"$f":"F6547*(1-Elteq!$F$9)","v":2.6720999365376263},"3501170898161"]
["TECHNIK","DYMO 1540",null,"S0720010 DYMO mechanický štítkovač profi, pro pásky šíře 9mm, výška tisku 5,1mm","1ks",62.348998519211285,{"$f":"F6548*(1-Elteq!$F$9)","v":62.348998519211285},"5411313540001"]
["TECHNIK","DYMO adaptér 9V",null,"S0721440 DYMO síťový adaptér 220V k přístrojům LM160, 210D, 220P, 450D, 500TS, RhinoPro, LetraTag","1ks",29.875561790455407,{"$f":"F6549*(1-Elteq!$F$9)","v":29.875561790455407},"5411313400763"]
["TECHNIK","DYMO adaptér12V",null,"S0895890 DYMO síťový adaptér 220V k přístrojům LM260P, 360D, 420P a PnP","1ks",29.875561790455407,{"$f":"F6550*(1-Elteq!$F$9)","v":29.875561790455407},"8591735038786"]
["TECHNIK","DYMO baterie",null,"1758458 DYMO dobíjecí baterie Li-Ion 7,4V / 650mA k tiskárnám LM260P, LM280 a LM PnP","1ks",21.896374479961107,{"$f":"F6551*(1-Elteq!$F$9)","v":21.896374479961107},""]
["TECHNIK","DYMO Junior",null,"S0717900 DYMO mechanický plastový štítkovač hobby pro pásky šíře 9mm, výška tisku 3mm","1ks",6.6802498413440663,{"$f":"F6552*(1-Elteq!$F$9)","v":6.6802498413440663},"5411313127462"]
["TECHNIK","DYMO M11",null,"S0720090 DYMO mechanický štítkovač Embosser M1011, profi celokovový","1ks",336.05367951872512,{"$f":"F6553*(1-Elteq!$F$9)","v":336.05367951872512},"5411313011105"]
["TECHNIK","DYMO Omega",null,"S0717930 DYMO mechanický plastový štítkovač economy pro pásky šíře 9mm, výška tisku 3,7mm","1ks",9.2781247796445356,{"$f":"F6554*(1-Elteq!$F$9)","v":9.2781247796445356},"5411313127486"]
["TECHNIK","LetraTag MOMENTUM",null,"S0758400 DYMO elektronický štítkovač LT-100T pro pásky šíře 12mm","1ks",30.432249277234078,{"$f":"F6555*(1-Elteq!$F$9)","v":30.432249277234078},"5411313225625"]
["TECHNIK","LetraTag RAZOR",null,"S0884020 DYMO elektronický štítkovač LT-100H pro pásky šíře 12mm (dříve S0725620)","1ks",30.432249277234078,{"$f":"F6556*(1-Elteq!$F$9)","v":30.432249277234078},"3501170884027"]
["TECHNIK","LM 160",null,"S0946340 DYMO elektronický štítkovač pro pásky šíře 6, 9 a 12mm","1ks",33.77237419790611,{"$f":"F6557*(1-Elteq!$F$9)","v":33.77237419790611},"3501170946343"]
["TECHNIK","LM 160+3",null,"1940295 DYMO elektronický štítkovač pro pásky šíře 6, 9 a 12mm + 3 pásky (45013, 45013, 45021)","1ks",56.039873669053001,{"$f":"F6558*(1-Elteq!$F$9)","v":56.039873669053001},""]
["TECHNIK","LM 210D",null,"S0784450 DYMO elektronický štítkovač pro pásky šíře 6, 9 a 12mm","1ks",46.947311385001356,{"$f":"F6559*(1-Elteq!$F$9)","v":46.947311385001356},"3501170784457"]
["TECHNIK","LM 280",null,"S0968940 DYMO štítkovač pro pásky šíře 6, 9 a 12mm, propojitelný s PC přes USB","1ks",67.17362340462644,{"$f":"F6560*(1-Elteq!$F$9)","v":67.17362340462644},""]
["TECHNIK","LM 280+4",null,"1921658 DYMO elektronický štítkovač propojitelný s PC / USB + 4 pásky (45010, 45013, 45017, 45021)","1ks",110.96637236454866,{"$f":"F6561*(1-Elteq!$F$9)","v":110.96637236454866},""]
["TECHNIK","LM 360D",null,"S0879500 DYMO elektronický štítkovač pro pásky šíře 6, 9, 12 a 19mm","1ks",111.89418484251311,{"$f":"F6562*(1-Elteq!$F$9)","v":111.89418484251311},"3501170879504"]
["TECHNIK","LM 420P",null,"S0915470 DYMO elektronický štítkovač pro pásky šíře 6, 9, 12 a 19mm, propojitelný s PC přes USB","1ks",128.40924695028039,{"$f":"F6563*(1-Elteq!$F$9)","v":128.40924695028039},"3501170915479"]
["TECHNIK","LM 500TS",null,"S0946430 DYMO štítkovač pro pásky 6, 9, 12, 19 a 24mm, propojitelný s PC přes USB, dotykový displej","1ks",223.04611970265466,{"$f":"F6564*(1-Elteq!$F$9)","v":223.04611970265466},"3501170946435"]
["TECHNIK","LM PnP AKCE",null,"S0915360 DYMO štítkovač pro pásky šíře 6, 9 a 12mm, propojitelný s PC přes USB (dříve 1710 Kč)","1ks",33.030124215534549,{"$f":"F6565*(1-Elteq!$F$9)","v":33.030124215534549},"3501170915363"]
["TECHNIK","LM PnP wireless",null,"S0969030 DYMO štítkovač pro pásky šíře 6, 9, 12, 19 a 24mm, propojitelný s PC přes USB a Wifi","1ks",134.34724680925288,{"$f":"F6566*(1-Elteq!$F$9)","v":134.34724680925288},""]
["TECHNIK","LM PnP+2",null,"1903842 DYMO elektronický štítkovač propojitelný s PC přes USB + pásky 40918, 45013","1ks",37.817636601831133,{"$f":"F6567*(1-Elteq!$F$9)","v":37.817636601831133},""]
["TECHNIK","LW 450",null,"S0838780 DYMO elektronická tiskárna štítků, 600x300dpi, šíře tisku 56mm, USB","1ks",127.11030948113014,{"$f":"F6568*(1-Elteq!$F$9)","v":127.11030948113014},"3501170838785"]
["TECHNIK","LW 450 Duo",null,"S0838930 DYMO elektronická tiskárna štítků, 600x300dpi, šíře tisku 56mm, USB","1ks",218.03593232164661,{"$f":"F6569*(1-Elteq!$F$9)","v":218.03593232164661},"3501170838938"]
["TECHNIK","LW 450 Turbo",null,"S0838830 DYMO elektronická tiskárna štítků, 600x300dpi, šíře tisku 56mm, USB","1ks",163.48055861733673,{"$f":"F6570*(1-Elteq!$F$9)","v":163.48055861733673},"3501170838839"]
["TECHNIK","LW 450 Twin",null,"S0838880 DYMO elektronická tiskárna štítků, 600x300dpi, šíře tisku 56mm, USB","1ks",222.1183072246902,{"$f":"F6571*(1-Elteq!$F$9)","v":222.1183072246902},"3501170838884"]
["TECHNIK","LW 4XL",null,"S0904950 DYMO elektronická tiskárna štítků, 300dpi, šíře tisku 106mm, USB","1ks",327.88892971263795,{"$f":"F6572*(1-Elteq!$F$9)","v":327.88892971263795},"3501170904961"]
["TECHNIK","PL 150",null,"RhinoPRO 4200 štítkovač s elektrosymboly pro pásky 6,9,12 a 19mm","1ks",89.441122875773331,{"$f":"F6573*(1-Elteq!$F$9)","v":89.441122875773331},"3501170955987"]
["TECHNIK","PL 150 K",null,"RhinoPRO 4200 SET štítkovač s elektrosymboly pro pásky 6,9,12 a 19mm, vč. kufru","1ks",111.15193486014155,{"$f":"F6574*(1-Elteq!$F$9)","v":111.15193486014155},""]
["TECHNIK","PL 200",null,"RhinoPRO 5200 štítkovač s elektrosymboly pro pásky 6,9,12 a 19mm","1ks",176.2843708132462,{"$f":"F6575*(1-Elteq!$F$9)","v":176.2843708132462},"3501170841495"]
["TECHNIK","PL 200 baterie",null,"Dobíjecí baterie 7,4V/1400mAh k tiskárnám LM360D, PL150 a PL200 (dříve RhinoPRO 4200 a 5200)","1ks",29.875561790455407,{"$f":"F6576*(1-Elteq!$F$9)","v":29.875561790455407},"3501170895849"]
["TECHNIK","PL 200 K",null,"RhinoPRO 5200 SET štítkovač s elektrosymboly pro pásky 6,9,12 a 19mm","1ks",235.10768191619255,{"$f":"F6577*(1-Elteq!$F$9)","v":235.10768191619255},"3501170841433"]
["TECHNIK","PL 200 kufřík",null,"Plastový kufřík k tiskárně PL200 (dříve k tiskárně RhinoPRO 5200)","1ks",23.937561931482904,{"$f":"F6578*(1-Elteq!$F$9)","v":23.937561931482904},"3501170902394"]
["TECHNIK","PL 300",null,"RhinoPRO 6000 štítkovač s elektrosymboly pro pásky 6,9,12,19 a 24mm","1ks",293.9309930191389,{"$f":"F6579*(1-Elteq!$F$9)","v":293.9309930191389},""]
["TECHNIK","PL 300 baterie",null,"Dobíjecí baterie k tiskárně PL300 (dříve RhinoPRO 6000)","1ks",29.875561790455407,{"$f":"F6580*(1-Elteq!$F$9)","v":29.875561790455407},"8591735037055"]
["TECHNIK","PL 300 K",null,"RhinoPRO 6000 SET štítkovač s elektrosymboly pro pásky 6 až 24mm","1ks",411.20649023384584,{"$f":"F6581*(1-Elteq!$F$9)","v":411.20649023384584},""]
["TECHNIK","RHINO 101-K",null,"S0810290 DYMO RHINO zásobník se samolepicími štítky na kabely 19x38/19x12mm (140 štítků)","1ks",19.112937046067746,{"$f":"F6582*(1-Elteq!$F$9)","v":19.112937046067746},""]
["TECHNIK","RHINO 101-O",null,"S0810250 DYMO RHINO zásobník s bílou samolepicí páskou 19mm, návin 3,5m","1ks",19.112937046067746,{"$f":"F6583*(1-Elteq!$F$9)","v":19.112937046067746},""]
["TECHNIK","S0719250",null,"14681 DYMO štítky na CD/DVD papírové průměr 57mm, bílé (balení 160ks etiket)","1ks",12.247124709130787,{"$f":"F6584*(1-Elteq!$F$9)","v":12.247124709130787},"5411313146814"]
["TECHNIK","S0722370",null,"99010 DYMO adresní štítky papírové 89x28mm, bílé (balení 2x130ks etiket)","1ks",11.875999717945007,{"$f":"F6585*(1-Elteq!$F$9)","v":11.875999717945007},"5411313990103"]
["TECHNIK","S0722380",null,"99011 DYMO adresní štítky papírové 89x28mm, mix barev (balení 4x130ks etiket)","1ks",39.339249065692833,{"$f":"F6586*(1-Elteq!$F$9)","v":39.339249065692833},"5411313990110"]
["TECHNIK","S0722400",null,"99012 DYMO adresní štítky papírové 89x36mm, bílé (balení 2x260ks etiket)","1ks",23.751999435890014,{"$f":"F6587*(1-Elteq!$F$9)","v":23.751999435890014},"5411313990127"]
["TECHNIK","S0722410",null,"99013 DYMO adresní štítky plastové 89x36mm, průhledné (balení 260ks etiket)","1ks",26.720999365376265,{"$f":"F6588*(1-Elteq!$F$9)","v":26.720999365376265},"5411313990134"]
["TECHNIK","S0722430",null,"99014 DYMO jmenovky papírové 101x54mm, bílé (balení 220ks etiket)","1ks",20.040749524032197,{"$f":"F6589*(1-Elteq!$F$9)","v":20.040749524032197},"5411313990141"]
["TECHNIK","S0722440",null,"99015 DYMO štítky na diskety papírové 70x54mm, bílé (balení 320ks etiket)","1ks",22.824186957925559,{"$f":"F6590*(1-Elteq!$F$9)","v":22.824186957925559},"5411313990158"]
["TECHNIK","S0722460",null,"99017 DYMO štítky na závěsné desky 50x12mm, bílé (balení 220ks etiket)","1ks",12.247124709130787,{"$f":"F6591*(1-Elteq!$F$9)","v":12.247124709130787},"5411313990172"]
["TECHNIK","S0722470",null,"99018 DYMO štítky na pořadače papírové 38x190mm, bílé (balení 110ks etiket)","1ks",22.453061966739778,{"$f":"F6592*(1-Elteq!$F$9)","v":22.453061966739778},"5411313990189"]
["TECHNIK","S0722480",null,"99019 DYMO štítky na pořadače papírové 59x190mm, bílé (balení 110ks etiket)","1ks",28.019936834526501,{"$f":"F6593*(1-Elteq!$F$9)","v":28.019936834526501},"5411313990196"]
["TECHNIK","S0722520",null,"11352 DYMO multifunkční štítky papírové 25x54mm, bílé (balení 500ks etiket)","1ks",10.762624744387661,{"$f":"F6594*(1-Elteq!$F$9)","v":10.762624744387661},"5411313113526"]
["TECHNIK","S0722530",null,"11353 DYMO multifunkční štítky papírové 24x12mm, bílé (balení 1000ks etiket)","1ks",9.649249770830318,{"$f":"F6595*(1-Elteq!$F$9)","v":9.649249770830318},"5411313113533"]
["TECHNIK","S0722540",null,"11354 DYMO multifunkční štítky papírové 57x32mm, bílé (balení 1000ks etiket)","1ks",25.050936905040249,{"$f":"F6596*(1-Elteq!$F$9)","v":25.050936905040249},"5411313113540"]
["TECHNIK","S0722550",null,"11355 DYMO multifunkční štítky papírové 19x51mm, bílé (balení 500ks etiket)","1ks",11.504874726759224,{"$f":"F6597*(1-Elteq!$F$9)","v":11.504874726759224},"5411313113557"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK"},"S0722560",null,"11356 DYMO adresní štítky papírové 89x41mm, bílé (balení 300ks etiket)","1ks",19.112937046067746,{"$f":"F6598*(1-Elteq!$F$9)","v":19.112937046067746},"5411313113564"]
["TECHNIK","S0904980",null,"Extra velké štítky papírové XXL 159x104mm, bílé","1ks",26.720999365376265,{"$f":"F6599*(1-Elteq!$F$9)","v":26.720999365376265},"3501170904985"]
["TECHNIK","M-3E páska 30mm Č",null,"Tisková páska k tiskovým kleštím HOTMARKER M-3E, šíře 30mm, návin 50m","1ks",35.25687416264924,{"$f":"F6600*(1-Elteq!$F$9)","v":35.25687416264924},"8591735054298"]
["TECHNIK","M-3E páska 35mm Č",null,"Tisková páska k tiskovým kleštím HOTMARKER M-3E, šíře 35mm, návin 50m","1ks",35.25687416264924,{"$f":"F6601*(1-Elteq!$F$9)","v":35.25687416264924},"8591735038724"]
["TECHNIK","92-BLK-PR443U",null,"Páska KROY šíře 110mm, barvící páska černá, návin 00m","1ks",59.379998589725034,{"$f":"F6602*(1-Elteq!$F$9)","v":59.379998589725034},""]
["TECHNIK","94-7872-C425",null,"Páska KROY šíře 100mm, platinová, návin 40m","1ks",76.822873175456763,{"$f":"F6603*(1-Elteq!$F$9)","v":76.822873175456763},""]
["TECHNIK","98-WT31-1242",null,"Smršťovací trubice KROY 2:1 průměr 12,7mm, návin 30m, barva bílá","1ks",32.658999224348769,{"$f":"F6604*(1-Elteq!$F$9)","v":32.658999224348769},""]

{"sheet":"TECHNIK SPECIAL - AKCIA","index":8,"n_rows":6362,"n_cols":8,"rows_kept":6362,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["sheetname","Objednávací kód",null,"Popis","Balenie","Cena za ks alebo m","Cena za kus po zľave","EAN"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK SPECIAL - AKCIA"},"AHP 03",null,"03853 ALFRA hydraulické čerpadlo na síť 220V s tlakovou hadicí délky 2m","1ks",2536.8248772504094,{"$f":"F5*(1-Elteq!$F$10)","v":2536.8248772504094},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK SPECIAL - AKCIA"},"ANP 8 STD",null,"Hydraulické čerpadlo na síť 220V s tlakem 20-850 bar, s tlakovou hadicí 3m","1ks",3374.268419861125,{"$f":"F6*(1-Elteq!$F$10)","v":3374.268419861125},""]
["TECHNIK SPECIAL - AKCIA","B70M-P24",null,"Hydraulické čerpadlo na baterie 24V s tlakem 700 bar, vč. nabíječky, brašny a tlakové hadice 3m","1ks",3656.323413162319,{"$f":"F7*(1-Elteq!$F$10)","v":3656.323413162319},""]
["TECHNIK SPECIAL - AKCIA","BP 1",null,"Hydraulické čerpadlo benzínové 700bar / 2,2kW / 25kg / 0,65-2,2 l/min. bez podstavce","1ks",3927.6157817191252,{"$f":"F8*(1-Elteq!$F$10)","v":3927.6157817191252},""]
["TECHNIK SPECIAL - AKCIA","BP 3",null,"Hydraulické čerpadlo benzínové 700bar / 3,2kW / 60kg / 610x470x850mm / 1,2-4,3 l/min. s podstavcem","1ks",3799.5776597600307,{"$f":"F9*(1-Elteq!$F$10)","v":3799.5776597600307},""]
["TECHNIK SPECIAL - AKCIA","DSP 120",null,"02027 ALFRA hydraulické čerpadlo na síť 220V s tlakovou hadicí délky 1,8m","1ks",2990.7107414706197,{"$f":"F10*(1-Elteq!$F$10)","v":2990.7107414706197},""]
["TECHNIK SPECIAL - AKCIA","DSP 120 nožní ovl.  ",null,"02029 ALFRA nožní ovládání k čerpadlu DSP120","1ks",211.54124497589544,{"$f":"F11*(1-Elteq!$F$10)","v":211.54124497589544},""]
["TECHNIK SPECIAL - AKCIA","EHP 1",null,"Hydraulické čerpadlo na síť 220V s tlakovou hadicí 2m vč. plastového kufru","1ks",1835.2130814136892,{"$f":"F12*(1-Elteq!$F$10)","v":1835.2130814136892},""]
["TECHNIK SPECIAL - AKCIA","FP 700",null,"Hydraulické nožní čerpadlo s tlakem 700 bar, vč. brašny a tlakové hadice 3m","1ks",858.78322960389835,{"$f":"F13*(1-Elteq!$F$10)","v":858.78322960389835},""]
["TECHNIK SPECIAL - AKCIA","FP 850",null,"Hydraulické nožní čerpadlo s tlakem 850 bar, vč. brašny a tlakové hadice 3m","1ks",902.20485357263476,{"$f":"F14*(1-Elteq!$F$10)","v":902.20485357263476},""]
["TECHNIK SPECIAL - AKCIA","FPA 700",null,"02121 ALFRA hydraulické nožní čerpadlo s tlakem 700 bar, vč. tlakové hadice 2,8m","1ks",850.43291730221824,{"$f":"F15*(1-Elteq!$F$10)","v":850.43291730221824},""]
["TECHNIK SPECIAL - AKCIA","HAD 2",null,"Hydraulická hadice 2m oboustranně osazená rychlospojkami CEJN","1ks",209.68562001996654,{"$f":"F16*(1-Elteq!$F$10)","v":209.68562001996654},""]
["TECHNIK SPECIAL - AKCIA","HAD 3",null,"Hydraulická hadice 3m oboustranně osazená rychlospojkami CEJN","1ks",234.55099442941389,{"$f":"F17*(1-Elteq!$F$10)","v":234.55099442941389},""]
["TECHNIK SPECIAL - AKCIA","HAD 5",null,"Hydraulická hadice 5m oboustranně osazená rychlospojkami CEJN","1ks",282.05499330119392,{"$f":"F18*(1-Elteq!$F$10)","v":282.05499330119392},""]
["TECHNIK SPECIAL - AKCIA","HAD10",null,"Hydraulická hadice 10m oboustranně osazená rychlospojkami CEJN","1ks",552.97623686681436,{"$f":"F19*(1-Elteq!$F$10)","v":552.97623686681436},""]
["TECHNIK SPECIAL - AKCIA","NP7-700",null,"Hydraulické čerpadlo na síť 220V s tlakem 700 bar, bez tlakové hadice","1ks",3841.1436587728381,{"$f":"F20*(1-Elteq!$F$10)","v":3841.1436587728381},""]
["TECHNIK SPECIAL - AKCIA","NP7-850",null,"Hydraulické čerpadlo na síť 220V s tlakem 850 bar, bez tlakové hadice","1ks",3918.3376569394804,{"$f":"F21*(1-Elteq!$F$10)","v":3918.3376569394804},""]
["TECHNIK SPECIAL - AKCIA","OLEJ HF-E15",null,"Hydraulický olej typ SHELL Naturelle HF-E15 pro hydraulické nářadí (5 litrů)","1ks",89.069997884587551,{"$f":"F22*(1-Elteq!$F$10)","v":89.069997884587551},""]
["TECHNIK SPECIAL - AKCIA","OLEJ H-LP46",null,"01455 ALFRA hydraulický olej typ H-LP46 pro hydraulické nářadí (1 litr)","1ks",18.370687063696181,{"$f":"F23*(1-Elteq!$F$10)","v":18.370687063696181},""]
["TECHNIK SPECIAL - AKCIA","PO 7000",null,"Hydraulické nožní čerpadlo s tlakem 700 bar, vč. plastového kufru a tlakové hadice 3m","1ks",933.37935283224033,{"$f":"F24*(1-Elteq!$F$10)","v":933.37935283224033},""]
["TECHNIK SPECIAL - AKCIA","SC 05",null,"03852 ALFRA hydraulické čerpadlo na síť 220V s tlakovou hadicí délky 2m","1ks",5120.0403783990414,{"$f":"F25*(1-Elteq!$F$10)","v":5120.0403783990414},""]
["TECHNIK SPECIAL - AKCIA","V 24/230 UNI-F",null,"Hydraulické čerpadlo na síť i baterie 24V / 230V UNI FUTURE 2050 DA, bez tlakové hadice","1ks",5377.2299972907877,{"$f":"F26*(1-Elteq!$F$10)","v":5377.2299972907877},""]
["TECHNIK SPECIAL - AKCIA","ALFRA 03910",null,"03910 ALFRA hydraulický základní přístroj komplet s čerpadlem SC05","1ks",11063.792674734925,{"$f":"F27*(1-Elteq!$F$10)","v":11063.792674734925},""]
["TECHNIK SPECIAL - AKCIA","B 200",null,"03750 ALFRA hydraulická ohýbací hlavice pro pasovinu Cu 200x10mm a Al 200x16mm","1ks",37112.462006079026,{"$f":"F28*(1-Elteq!$F$10)","v":37112.462006079026},""]
["TECHNIK SPECIAL - AKCIA","BS 160",null,"03258 ALFRA hydraulická ohýbací a děrovací hlavice pro pasovinu Al a Cu 160x12mm","1ks",2280.563070836627,{"$f":"F29*(1-Elteq!$F$10)","v":2280.563070836627},""]
["TECHNIK SPECIAL - AKCIA","BS 160/R5",null,"03259 ALFRA razník s poloměrem R5 pro ohýbání do síly materiálu 8mm k hlavici BS160","1ks",289.84861811609534,{"$f":"F30*(1-Elteq!$F$10)","v":289.84861811609534},""]
["TECHNIK SPECIAL - AKCIA","BW 200",null,"Hydraulická ohýbací hlavice pro pasovinu Cu 200x13mm a Al 200x13mm","1ks",798.28985604061597,{"$f":"F31*(1-Elteq!$F$10)","v":798.28985604061597},""]
["TECHNIK SPECIAL - AKCIA","DP100Z PLUS",null,"Hydraulická děrovací hlavice pro AL a CU materiály s maximálními rozměry 100x10mm","1ks",855.99979217000498,{"$f":"F32*(1-Elteq!$F$10)","v":855.99979217000498},""]
["TECHNIK SPECIAL - AKCIA","ECW-H3D",null,"Hydraulická lisovací hlavice do 500mm2 (RH230)","1ks",606.97492308434562,{"$f":"F33*(1-Elteq!$F$10)","v":606.97492308434562},""]
["TECHNIK SPECIAL - AKCIA","LH 130",null,"Hydraulická lisovací hlavice do 240mm2","1ks",607.90273556231,{"$f":"F34*(1-Elteq!$F$10)","v":607.90273556231},""]
["TECHNIK SPECIAL - AKCIA","LH 130K",null,"Hydraulická lisovací hlavice do 240mm2 v kufru s příslušenstvím","1ks",887.35985392520342,{"$f":"F35*(1-Elteq!$F$10)","v":887.35985392520342},""]
["TECHNIK SPECIAL - AKCIA","LPV 120/12",null,"03256 ALFRA hydraulická stanice pro ohýbání a děrování pasovin Al a Cu 120x12mm","1ks",3398.5771067837936,{"$f":"F36*(1-Elteq!$F$10)","v":3398.5771067837936},""]
["TECHNIK SPECIAL - AKCIA","NC 1319",null,"Hydraulický střihač matek pro šroubové spoje M6 - M12","1ks",544.62592456513426,{"$f":"F37*(1-Elteq!$F$10)","v":544.62592456513426},""]
["TECHNIK SPECIAL - AKCIA","NC 1924",null,"Hydraulický střihač matek pro šroubové spoje M12 - M16","1ks",1074.0357244916515,{"$f":"F38*(1-Elteq!$F$10)","v":1074.0357244916515},""]
["TECHNIK SPECIAL - AKCIA","NC 2432",null,"Hydraulický střihač matek pro šroubové spoje M16 - M22","1ks",1342.1735306233786,{"$f":"F39*(1-Elteq!$F$10)","v":1342.1735306233786},""]
["TECHNIK SPECIAL - AKCIA","NC 3241",null,"Hydraulický střihač matek pro šroubové spoje M22 - M27","1ks",1589.528337248702,{"$f":"F40*(1-Elteq!$F$10)","v":1589.528337248702},""]
["TECHNIK SPECIAL - AKCIA","NP 100 U",null,"Hydraulická střihací hlavice na pasovinu","1ks",861.75222953338459,{"$f":"F41*(1-Elteq!$F$10)","v":861.75222953338459},""]
["TECHNIK SPECIAL - AKCIA","OP 100 D",null,"Hydraulická ohýbací hlavice pro pasovinu Al a Cu 100x10mm","1ks",1038.4077253378166,{"$f":"F42*(1-Elteq!$F$10)","v":1038.4077253378166},""]
["TECHNIK SPECIAL - AKCIA","OP 200",null,"Hydraulická ohýbací hlavice pro pasovinu Al a Cu 200x15mm","1ks",1288.9170943882191,{"$f":"F43*(1-Elteq!$F$10)","v":1288.9170943882191},""]
["TECHNIK SPECIAL - AKCIA","P 60 CK",null,"Hydraulická lisovací hlavice do 300mm2","1ks",612.72736044772523,{"$f":"F44*(1-Elteq!$F$10)","v":612.72736044772523},""]
["TECHNIK SPECIAL - AKCIA","PPV 120/12",null,"03200 ALFRA hydraulická stanice pro ohýbání a děrování pasovin Al a Cu 120x12mm","1ks",4943.3848825946088,{"$f":"F45*(1-Elteq!$F$10)","v":4943.3848825946088},""]
["TECHNIK SPECIAL - AKCIA","PPV 120/12 DD",null,"03203 ALFRA délkový doraz s jemným nastavením","1ks",379.66086598305441,{"$f":"F46*(1-Elteq!$F$10)","v":379.66086598305441},""]
["TECHNIK SPECIAL - AKCIA","PPV 120/12 DMS",null,"03229 ALFRA digitální měřicí systém úhlu ohybu s připojovacím kabelem","1ks",2000.9203899781407,{"$f":"F47*(1-Elteq!$F$10)","v":2000.9203899781407},""]
["TECHNIK SPECIAL - AKCIA","PPV 120/12 MMS",null,"03201 ALFRA mechanický měřící systém úhlu ohybu s připojovacím kabelem","1ks",303.20911779878344,{"$f":"F48*(1-Elteq!$F$10)","v":303.20911779878344},""]
["TECHNIK SPECIAL - AKCIA","PPV 120/12 OM",null,"03202 ALFRA ohybová matrice","1ks",351.64092914852796,{"$f":"F49*(1-Elteq!$F$10)","v":351.64092914852796},""]
["TECHNIK SPECIAL - AKCIA","PPV 160/10",null,"03200SET ALFRA hydraulická stanice pro ohýbání a děrování pasovin Al a Cu 160x10mm","1ks",8530.1223599095938,{"$f":"F50*(1-Elteq!$F$10)","v":8530.1223599095938},""]
["TECHNIK SPECIAL - AKCIA","RH 50",null,"Hydraulická lisovací hlavice do 185mm2","1ks",408.2374903043596,{"$f":"F51*(1-Elteq!$F$10)","v":408.2374903043596},""]
["TECHNIK SPECIAL - AKCIA","RHC 131",null,"Hydraulická lisovací hlavice do 300mm2","1ks",447.76230186564533,{"$f":"F52*(1-Elteq!$F$10)","v":447.76230186564533},"8591735040963"]
["TECHNIK SPECIAL - AKCIA","RHC 131 LN",null,"Hydraulická lisovací hlavice do 300mm2","1ks",531.82211236922478,{"$f":"F53*(1-Elteq!$F$10)","v":531.82211236922478},"8591735040970"]
["TECHNIK SPECIAL - AKCIA","RHM 132",null,"Hydraulická lisovací hlavice do 300mm2","1ks",624.04667267889147,{"$f":"F54*(1-Elteq!$F$10)","v":624.04667267889147},""]
["TECHNIK SPECIAL - AKCIA","RHT 160",null,"Hydraulická děrovací hlavice pro otvory 6,5-21,0mm pro otvory do 27,5mm od okraje pasoviny","1ks",796.43423108468699,{"$f":"F55*(1-Elteq!$F$10)","v":796.43423108468699},""]
["TECHNIK SPECIAL - AKCIA","RHT 160-60N",null,"Hydraulická děrovací hlavice pro otvory 6,5-21,0mm pro otvory do 55,0mm od okraje pasoviny","1ks",1273.7009697496019,{"$f":"F56*(1-Elteq!$F$10)","v":1273.7009697496019},""]
["TECHNIK SPECIAL - AKCIA","RHU 131-C",null,"Hydraulická lisovací hlavice do průřezu 300mm2","1ks",556.68748677867222,{"$f":"F57*(1-Elteq!$F$10)","v":556.68748677867222},""]
["TECHNIK SPECIAL - AKCIA","RHU 450",null,"Hydraulická lisovací hlavice do průřezu 1000mm2","1ks",964.55385209184601,{"$f":"F58*(1-Elteq!$F$10)","v":964.55385209184601},"8591735042721"]
["TECHNIK SPECIAL - AKCIA","RHU 520",null,"Hydraulická lisovací hlavice do průřezu 1200mm2","1ks",1257.3714701374277,{"$f":"F59*(1-Elteq!$F$10)","v":1257.3714701374277},""]
["TECHNIK SPECIAL - AKCIA","RHU1000",null,"Hydraulická lisovací hlavice do průřezu 2500mm2","1ks",6381.8653484306978,{"$f":"F60*(1-Elteq!$F$10)","v":6381.8653484306978},""]
["TECHNIK SPECIAL - AKCIA","S 125",null,"03250 ALFRA hydraulická střihací hlavice na pasovinu 120x12mm (SP120)","1ks",2148.0714489833031,{"$f":"F61*(1-Elteq!$F$10)","v":2148.0714489833031},""]
["TECHNIK SPECIAL - AKCIA","SK 130",null,"Kovový kufr pro čelisti typu C","1ks",153.08905886413484,{"$f":"F62*(1-Elteq!$F$10)","v":153.08905886413484},""]
["TECHNIK SPECIAL - AKCIA","SK 130 PL",null,"Plastový kufr pro uložení hlavice RH 131 a lisovacích čelistí","1ks",29.318874303676736,{"$f":"F63*(1-Elteq!$F$10)","v":29.318874303676736},"8591735046767"]
["TECHNIK SPECIAL - AKCIA","SK 130 U",null,"Kovový kufr pro uložení hlavice RHU 131 a lisovacích čelistí typu C","1ks",174.79987084850308,{"$f":"F64*(1-Elteq!$F$10)","v":174.79987084850308},""]
["TECHNIK SPECIAL - AKCIA","SK 230",null,"Kovový kufr pro hlavici ECW-H3D a RH230 (MK230)","1ks",128.40924695028039,{"$f":"F65*(1-Elteq!$F$10)","v":128.40924695028039},""]
["TECHNIK SPECIAL - AKCIA","SK 50 PL",null,"Plastový kufr pro hlavici RH 50","1ks",35.25687416264924,{"$f":"F66*(1-Elteq!$F$10)","v":35.25687416264924},""]
["TECHNIK SPECIAL - AKCIA","SK 520",null,"Kovový kufr pro hlavici RHU 450 a RHU 520 (MK450)","1ks",107.44068494828373,{"$f":"F67*(1-Elteq!$F$10)","v":107.44068494828373},""]
["TECHNIK SPECIAL - AKCIA","SK 520 C",null,"Kovový kufr pro čelisti k RHU 450 a RHU 520","1ks",145.48099654482633,{"$f":"F68*(1-Elteq!$F$10)","v":145.48099654482633},""]
["TECHNIK SPECIAL - AKCIA","AP  35/2",null,"Elektrohydraulické lisovací kleště do 120mm2, síla 35kN, vč.kufru, nabíječky a akumulátoru 18V/1,5Ah","1ks",1284.0924695028039,{"$f":"F69*(1-Elteq!$F$10)","v":1284.0924695028039},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK SPECIAL - AKCIA"},"AP  62",null,"Elektrohydraulické lisovací kleště do 300mm2, síla 62kN, vč.kufru, nabíječky a akumulátoru 18V/1,5Ah","1ks",1465.9437151838367,{"$f":"F70*(1-Elteq!$F$10)","v":1465.9437151838367},"8591735047634"]
["TECHNIK SPECIAL - AKCIA","AP  62 D",null,"Elektrohydraulické lisovací kleště do 300mm2, síla 62kN, vč. kufru, nabíječky a akumulátoru 18V/4Ah","1ks",1888.2839551532561,{"$f":"F71*(1-Elteq!$F$10)","v":1888.2839551532561},"8591735047641"]
["TECHNIK SPECIAL - AKCIA","AP 130",null,"Elektrohydraulické lisovací kleště do 400mm2, síla 130kN, vč. kufru, nabíječky a akumulátoru 18V/2Ah","1ks",1707.1749594545947,{"$f":"F72*(1-Elteq!$F$10)","v":1707.1749594545947},""]
["TECHNIK SPECIAL - AKCIA","AP 132 C26",null,"Elektrohydraulické lisovací kleště do 400mm2, síla 130kN, vč. kufru, nabíječky a akumulátoru 18V/4Ah","1ks",2042.671951486541,{"$f":"F73*(1-Elteq!$F$10)","v":2042.671951486541},"8591735047689"]
["TECHNIK SPECIAL - AKCIA","AP 132 C32",null,"Elektrohydraulické lisovací kleště do 400mm2, síla 130kN, vč. kufru, nabíječky a akumulátoru 18V/4Ah","1ks",2071.6197007990322,{"$f":"F74*(1-Elteq!$F$10)","v":2071.6197007990322},"8591735047696"]
["TECHNIK SPECIAL - AKCIA","AP 132 C38",null,"Elektrohydraulické lisovací kleště do 400mm2, síla 130kN, vč. kufru, nabíječky a akumulátoru 18V/4Ah","1ks",2165.5143235690348,{"$f":"F75*(1-Elteq!$F$10)","v":2165.5143235690348},"8591735047658"]
["TECHNIK SPECIAL - AKCIA","AP 132 U",null,"Elektrohydraulické lisovací kleště do 400mm2, síla 130kN, vč. kufru, nabíječky a akumulátoru 18V/4Ah","1ks",2304.6861952637028,{"$f":"F76*(1-Elteq!$F$10)","v":2304.6861952637028},"8591735047665"]
["TECHNIK SPECIAL - AKCIA","B 131-C",null,"Elektrohydraulické lisovací kleště do 400mm2, síla 130kN, vč. kufru, nabíječky a akumulátorů","1ks",2349.2211942059967,{"$f":"F77*(1-Elteq!$F$10)","v":2349.2211942059967},""]
["TECHNIK SPECIAL - AKCIA","B 131LN-C",null,"Elektrohydraulické lisovací kleště do 400mm2, síla 130kN, vč. kufru, nabíječky a akumulátorů","1ks",2478.0015661474627,{"$f":"F78*(1-Elteq!$F$10)","v":2478.0015661474627},""]
["TECHNIK SPECIAL - AKCIA","B 131-UC",null,"Elektrohydraulické lisovací kleště do 400mm2, síla 130kN, vč. kufru, nabíječky a akumulátorů","1ks",2491.3620658301511,{"$f":"F79*(1-Elteq!$F$10)","v":2491.3620658301511},""]
["TECHNIK SPECIAL - AKCIA","B 1350-C",null,"Elektrohydraulické lisovací kleště do 400mm2, síla 132kN, vč. kufru, nabíječky a akumulátorů 18V","1ks",2293.923570519315,{"$f":"F80*(1-Elteq!$F$10)","v":2293.923570519315},""]
["TECHNIK SPECIAL - AKCIA","B 1350L-C",null,"Elektrohydraulické lisovací kleště do 400mm2, síla 132kN, vč. kufru, nabíječky a akumulátorů 18V","1ks",2429.7553172933112,{"$f":"F81*(1-Elteq!$F$10)","v":2429.7553172933112},""]
["TECHNIK SPECIAL - AKCIA","B 1350-UC",null,"Elektrohydraulické lisovací kleště do 400mm2, síla 132kN, vč. kufru, nabíječky a akumulátorů 18V","1ks",2342.9120693558384,{"$f":"F82*(1-Elteq!$F$10)","v":2342.9120693558384},""]
["TECHNIK SPECIAL - AKCIA","B 15 D",null,"Elektrohydraulické lisovací kleště do 16mm2, síla 15kN, vč. kufru, nabíječky a akumulátorů","1ks",1349.7815929426872,{"$f":"F83*(1-Elteq!$F$10)","v":1349.7815929426872},""]
["TECHNIK SPECIAL - AKCIA","B 35-45 D",null,"Elektrohydraulické lisovací kleště do 120-150mm2, síla 35kN, vč. kufru, nabíječky a akumulátorů","1ks",1305.6177189915791,{"$f":"F84*(1-Elteq!$F$10)","v":1305.6177189915791},""]
["TECHNIK SPECIAL - AKCIA","B 35-50 D",null,"Elektrohydraulické lisovací kleště do 120-150mm2, síla 35kN, vč. kufru, nabíječky a akumulátorů","1ks",1399.5123417615819,{"$f":"F85*(1-Elteq!$F$10)","v":1399.5123417615819},""]
["TECHNIK SPECIAL - AKCIA","B 46",null,"Elektrohydraulické lisovací kleště do 120mm2, síla 50kN, vč. kufru, nabíječky a akumulátorů","1ks",1534.6018385532063,{"$f":"F86*(1-Elteq!$F$10)","v":1534.6018385532063},""]
["TECHNIK SPECIAL - AKCIA","B 500",null,"Elektrohydraulické lisovací kleště do 240mm2, síla 60kN, vč. kufru, nabíječky a akumulátorů (B51)","1ks",2338.4585694616089,{"$f":"F87*(1-Elteq!$F$10)","v":2338.4585694616089},""]
["TECHNIK SPECIAL - AKCIA","B 62",null,"Elektrohydraulické lisovací kleště do 240mm2, síla 60kN, vč. kufru, nabíječky a akumulátorů","1ks",1627.0119613584659,{"$f":"F88*(1-Elteq!$F$10)","v":1627.0119613584659},""]
["TECHNIK SPECIAL - AKCIA","BPS 230.14",null,"Síťový adaptér 230V / 14,4V pro napájení hydraulických bateriových zařízení","1ks",271.29236855680625,{"$f":"F89*(1-Elteq!$F$10)","v":271.29236855680625},""]
["TECHNIK SPECIAL - AKCIA","BPS 230.24",null,"Síťový adaptér 230V / 24V pro napájení hydraulických bateriových zařízení","1ks",295.41549298388202,{"$f":"F90*(1-Elteq!$F$10)","v":295.41549298388202},""]
["TECHNIK SPECIAL - AKCIA","EPG 10",null,"Elektrohydraulické lisovací kleště bateriové 13kN do průřezu 50mm2, Klauke EK15/50","1ks",1208.0118463097187,{"$f":"F91*(1-Elteq!$F$10)","v":1208.0118463097187},""]
["TECHNIK SPECIAL - AKCIA","EPG 15",null,"Elektrohydraulické lisovací kleště bateriové 13kN do průřezu 50mm2, Klauke EK15/50G","1ks",1255.3302826859058,{"$f":"F92*(1-Elteq!$F$10)","v":1255.3302826859058},""]
["TECHNIK SPECIAL - AKCIA","EPG 20",null,"Elektrohydraulické lisovací kleště bateriové 35kN do průřezu 120mm2, Klauke EK35/4","1ks",1208.0118463097187,{"$f":"F93*(1-Elteq!$F$10)","v":1208.0118463097187},""]
["TECHNIK SPECIAL - AKCIA","HK 60 22",null,"Hydraulické lisovací kleště do 300mm2 Klauke","1ks",1797.1727698171467,{"$f":"F94*(1-Elteq!$F$10)","v":1797.1727698171467},""]
["TECHNIK SPECIAL - AKCIA","HP 60 CK",null,"Hydraulické lisovací kleště do 300mm2 vč. plastového kufru","1ks",915.93647824650861,{"$f":"F95*(1-Elteq!$F$10)","v":915.93647824650861},""]
["TECHNIK SPECIAL - AKCIA","HT 131-C",null,"Hydraulické lisovací kleště do 300mm2 s hlavou typu \"C\" vč. plastového kufru","1ks",890.32885385468967,{"$f":"F96*(1-Elteq!$F$10)","v":890.32885385468967},""]
["TECHNIK SPECIAL - AKCIA","HT 131LN-C",null,"Hydraulické lisovací kleště do 300mm2 s prodlouženou hlavou typu \"C\" vč. plastového kufru","1ks",1011.6867259724403,{"$f":"F97*(1-Elteq!$F$10)","v":1011.6867259724403},""]
["TECHNIK SPECIAL - AKCIA","HT 131-UC",null,"Hydraulické lisovací kleště do 300mm2 s hlavou typu \"U\" vč. plastového kufru","1ks",1024.6761006639426,{"$f":"F98*(1-Elteq!$F$10)","v":1024.6761006639426},""]
["TECHNIK SPECIAL - AKCIA","HT 45E",null,"Hydraulické lisovací kleště do 120mm2 vč. plastového kufru","1ks",452.77248924665338,{"$f":"F99*(1-Elteq!$F$10)","v":452.77248924665338},""]
["TECHNIK SPECIAL - AKCIA","HT 51",null,"Hydraulické lisovací kleště do 240mm2 vč. plastového kufru","1ks",601.77917320774463,{"$f":"F100*(1-Elteq!$F$10)","v":601.77917320774463},""]
["TECHNIK SPECIAL - AKCIA","LKE1",null,"Lisovací kleště elektromechanické na kabelové koncovky - vč. kufru, nabíječky a akku, bez čelistí","1sada",1204.3005963978608,{"$f":"F101*(1-Elteq!$F$10)","v":1204.3005963978608},"8591735048617"]
["TECHNIK SPECIAL - AKCIA","K 18",null,"Mechanické lisovací kleště pro CU do 240mm2 a AL do 185mm2, bez kufru, bez čelistí (MHP6/185)","1ks",515.12148776586469,{"$f":"F102*(1-Elteq!$F$10)","v":515.12148776586469},"8591735023898"]
["TECHNIK SPECIAL - AKCIA","K 18 L",null,"Mechanické lisovací kleště pro CU do 240mm2 a AL do 185mm2 s kovovým kufrem, bez čelistí","1ks",370.38274120340992,{"$f":"F103*(1-Elteq!$F$10)","v":370.38274120340992},"8591735055622"]
["TECHNIK SPECIAL - AKCIA","K 22",null,"Mechanické lisovací kleště pro CU do 300mm2 a AL do 240mm2, bez kufru, bez čelistí (MHP10/240)","1ks",718.49798293567289,{"$f":"F104*(1-Elteq!$F$10)","v":718.49798293567289},"8591735023904"]
["TECHNIK SPECIAL - AKCIA","K 22 L",null,"Mechanické lisovací kleště pro CU do 300mm2 a AL do 240mm s kovovým kufrem, bez čelistí","1ks",589.34648600302091,{"$f":"F105*(1-Elteq!$F$10)","v":589.34648600302091},"8591735055639"]
["TECHNIK SPECIAL - AKCIA","SK 18",null,"Kovový kufr ke kleštím K 18","1ks",152.71793387294906,{"$f":"F106*(1-Elteq!$F$10)","v":152.71793387294906},"8591735025397"]
["TECHNIK SPECIAL - AKCIA","SK 22",null,"Kovový kufr ke kleštím K 22","1ks",142.51199661534008,{"$f":"F107*(1-Elteq!$F$10)","v":142.51199661534008},"8591735013172"]
["TECHNIK SPECIAL - AKCIA","FP brašna",null,"Brašna s popruhem přes rameno, profesionální, vyztužená, pro nožní čerpadlo FP700 a hlavici TC120","1ks",131.74937187095242,{"$f":"F108*(1-Elteq!$F$10)","v":131.74937187095242},""]
["TECHNIK SPECIAL - AKCIA","TRS-B70",null,"Ruksak na záda pro čerpadlo B70M-P24","1ks",106.69843496591217,{"$f":"F109*(1-Elteq!$F$10)","v":106.69843496591217},""]
["TECHNIK SPECIAL - AKCIA","TOOL SET 11",null,"Sada nářadí pro zpracování VN kabelů TOOLSET 11","1sada",1242.3409079944033,{"$f":"F110*(1-Elteq!$F$10)","v":1242.3409079944033},"8591735052331"]
["TECHNIK SPECIAL - AKCIA","TOOL SET 12",null,"Sada nářadí pro zpracování VN kabelů TOOLSET 12","1sada",1229.3515333029011,{"$f":"F111*(1-Elteq!$F$10)","v":1229.3515333029011},"8591735052348"]
["TECHNIK SPECIAL - AKCIA","AS 32",null,"Elektrohydraulické nůžky do průměru 32mm","1ks",1238.4440955869527,{"$f":"F112*(1-Elteq!$F$10)","v":1238.4440955869527},""]
["TECHNIK SPECIAL - AKCIA","AS 34",null,"Elektrohydraulické nůžky do průměru 34mm","1ks",1335.8644057732204,{"$f":"F113*(1-Elteq!$F$10)","v":1335.8644057732204},""]
["TECHNIK SPECIAL - AKCIA","AS 52",null,"Elektrohydraulické nůžky do průměru 50mm","1ks",1157.5388475084524,{"$f":"F114*(1-Elteq!$F$10)","v":1157.5388475084524},""]
["TECHNIK SPECIAL - AKCIA","BC 25",null,"Elektrohydraulické nůžky do průměru 25mm","1ks",1665.6089604417871,{"$f":"F115*(1-Elteq!$F$10)","v":1665.6089604417871},""]
["TECHNIK SPECIAL - AKCIA","BC 55",null,"Elektrohydraulické nůžky do průměru 55mm, kufr, nabíječka, 1x akku 18V Li-Ion","1ks",2253.0998214888791,{"$f":"F116*(1-Elteq!$F$10)","v":2253.0998214888791},""]
["TECHNIK SPECIAL - AKCIA","BC 85",null,"Elektrohydraulické nůžky do průměru 85mm, kufr, nabíječka, 1x akku 18V Li-Ion","1ks",2698.4498109118172,{"$f":"F117*(1-Elteq!$F$10)","v":2698.4498109118172},""]
["TECHNIK SPECIAL - AKCIA","BC 90",null,"Elektrohydraulické nůžky do průměru 90mm, kufr, nabíječka, 1x akku 18V Li-Ion","1ks",3237.6944231047573,{"$f":"F118*(1-Elteq!$F$10)","v":3237.6944231047573},""]
["TECHNIK SPECIAL - AKCIA","B-TC 026",null,"Elektrohydraulické nůžky do průměru 24mm","1ks",1854.8827059465357,{"$f":"F119*(1-Elteq!$F$10)","v":1854.8827059465357},""]
["TECHNIK SPECIAL - AKCIA","B-TC 04",null,"Elektrohydraulické nůžky do průměru 40mm","1ks",2835.9516201461488,{"$f":"F120*(1-Elteq!$F$10)","v":2835.9516201461488},""]
["TECHNIK SPECIAL - AKCIA","B-TC 051",null,"Elektrohydraulické nůžky do průměru 50mm, kufr, nabíječka, 2x akku 14,4V Li-Ion","1ks",1999.6214525089904,{"$f":"F121*(1-Elteq!$F$10)","v":1999.6214525089904},""]
["TECHNIK SPECIAL - AKCIA","B-TC 055",null,"Elektrohydraulické nůžky do průměru 55mm, dvoupístové s rychloposuvem, kufr, nabíječka, 2 akku 14,4V","1ks",2914.8156807731275,{"$f":"F122*(1-Elteq!$F$10)","v":2914.8156807731275},""]
["TECHNIK SPECIAL - AKCIA","B-TC 065",null,"Elektrohydraulické nůžky do průměru 65mm, kufr, nabíječka, 2x akku 14,4V Li-Ion","1ks",2308.5830076711536,{"$f":"F123*(1-Elteq!$F$10)","v":2308.5830076711536},""]
["TECHNIK SPECIAL - AKCIA","B-TC 095",null,"Elektrohydraulické nůžky do průměru 95mm","1ks",2801.0658709746854,{"$f":"F124*(1-Elteq!$F$10)","v":2801.0658709746854},""]
["TECHNIK SPECIAL - AKCIA","B-TC 650",null,"Elektrohydraulické nůžky do průměru 65mm, kufr, nabíječka, 2x akku 18V","1ks",2624.2248126746608,{"$f":"F125*(1-Elteq!$F$10)","v":2624.2248126746608},""]
["TECHNIK SPECIAL - AKCIA","HT-TC 026",null,"Hydraulické nůžky do průměru 25mm na AL, Cu kabely a ALFe lana","1ks",827.42316784869979,{"$f":"F126*(1-Elteq!$F$10)","v":827.42316784869979},""]
["TECHNIK SPECIAL - AKCIA","HT-TC 026 Y",null,"Hydraulické nůžky do průměru 25mm na AL, Cu kabely, ALFe a Fe lana","1ks",866.39129192320684,{"$f":"F127*(1-Elteq!$F$10)","v":866.39129192320684},""]
["TECHNIK SPECIAL - AKCIA","HT-TC 041",null,"Hydraulické nůžky do průměru 40mm na AL, Cu kabely a ALFe lana","1ks",1187.2288468033148,{"$f":"F128*(1-Elteq!$F$10)","v":1187.2288468033148},""]
["TECHNIK SPECIAL - AKCIA","HT-TC 051",null,"Hydraulické nůžky do průměru 50mm na AL a Cu kabely","1ks",919.83329065395935,{"$f":"F129*(1-Elteq!$F$10)","v":919.83329065395935},""]
["TECHNIK SPECIAL - AKCIA","HT-TC 055",null,"Hydraulické nůžky do průměru 55mm na AL a Cu kabely","1ks",1715.7108342518677,{"$f":"F130*(1-Elteq!$F$10)","v":1715.7108342518677},""]
["TECHNIK SPECIAL - AKCIA","HT-TC 065",null,"Hydraulické nůžky do průměru 65mm na AL a Cu kabely","1ks",1224.5269084174859,{"$f":"F131*(1-Elteq!$F$10)","v":1224.5269084174859},""]
["TECHNIK SPECIAL - AKCIA","HT-TC 0851",null,"Hydraulické nůžky do průměru 85mm na AL a Cu kabely vč. pouzdra","1ks",1357.9463427487744,{"$f":"F132*(1-Elteq!$F$10)","v":1357.9463427487744},""]
["TECHNIK SPECIAL - AKCIA","KN 40",null,"Hydraulická střihací hlavice do průměru 40mm","1ks",716.27123298855827,{"$f":"F133*(1-Elteq!$F$10)","v":716.27123298855827},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK SPECIAL - AKCIA"},"KN 65",null,"Hydraulická střihací hlavice do průměru 65mm","1ks",703.4674207926488,{"$f":"F134*(1-Elteq!$F$10)","v":703.4674207926488},""]
["TECHNIK SPECIAL - AKCIA","KN 85",null,"Hydraulická střihací hlavice do průměru 85mm","1ks",864.35010447168497,{"$f":"F135*(1-Elteq!$F$10)","v":864.35010447168497},""]
["TECHNIK SPECIAL - AKCIA","TC 025",null,"Hydraulická střihací hlavice do průměru 25mm, na AL, Cu a ALFe (síla 50kN)","1ks",666.16935917847775,{"$f":"F136*(1-Elteq!$F$10)","v":666.16935917847775},""]
["TECHNIK SPECIAL - AKCIA","TC 04",null,"Hydraulická střihací hlavice do průměru 40mm, na AL, Cu a ALFe (síla 100kN)","1ks",848.76285484188224,{"$f":"F137*(1-Elteq!$F$10)","v":848.76285484188224},""]
["TECHNIK SPECIAL - AKCIA","TC 045",null,"Hydraulická střihací hlavice do průměru 45mm, na AL, Cu a ALFe (síla 60 kN)","1ks",688.43685864962458,{"$f":"F138*(1-Elteq!$F$10)","v":688.43685864962458},""]
["TECHNIK SPECIAL - AKCIA","TC 050",null,"Hydraulická střihací hlavice do průměru 50mm, na AL, Cu (síla 50kN)","1ks",700.68398335875543,{"$f":"F139*(1-Elteq!$F$10)","v":700.68398335875543},""]
["TECHNIK SPECIAL - AKCIA","TC 055",null,"Hydraulická střihací hlavice do průměru 55mm, na AL, Cu","1ks",1421.2231537459502,{"$f":"F140*(1-Elteq!$F$10)","v":1421.2231537459502},""]
["TECHNIK SPECIAL - AKCIA","TC 085",null,"Hydraulická střihací hlavice do průměru 85mm, na AL, Cu (síla 56kN)","1ks",1017.9958508225985,{"$f":"F141*(1-Elteq!$F$10)","v":1017.9958508225985},""]
["TECHNIK SPECIAL - AKCIA","TC 096",null,"Hydraulická střihací hlavice do průměru 96mm, na AL, Cu (síla 85kN)","1ks",1228.7948458161225,{"$f":"F142*(1-Elteq!$F$10)","v":1228.7948458161225},""]
["TECHNIK SPECIAL - AKCIA","TC 120",null,"Hydraulická střihací hlavice do průměru 120mm, na AL, Cu (síla 110kN)","1ks",1448.500840598105,{"$f":"F143*(1-Elteq!$F$10)","v":1448.500840598105},""]
["TECHNIK SPECIAL - AKCIA","TC 120 kufr",null,"Kufr kovový pro střihací hlavici TC120","1ks",106.88399746150506,{"$f":"F144*(1-Elteq!$F$10)","v":106.88399746150506},""]
["TECHNIK SPECIAL - AKCIA","ALC/5,5",null,"03007 ALFRA razník s matricí do nůžek ALC na DIN lišty, kruhový otvor průměr 5,5mm","1ks",138.80074670348228,{"$f":"F145*(1-Elteq!$F$10)","v":138.80074670348228},""]
["TECHNIK SPECIAL - AKCIA","ALC/6",null,"03008 ALFRA razník s matricí do nůžek ALC na DIN lišty, kruhový otvor průměr 6,0mm","1ks",138.80074670348228,{"$f":"F146*(1-Elteq!$F$10)","v":138.80074670348228},""]
["TECHNIK SPECIAL - AKCIA","ALC/7",null,"03010 ALFRA razník s matricí do nůžek ALC na DIN lišty, kruhový otvor průměr 7,0mm","1ks",249.58155657243802,{"$f":"F147*(1-Elteq!$F$10)","v":249.58155657243802},""]
["TECHNIK SPECIAL - AKCIA","ALC/PO 12x6,4",null,"03005 ALFRA razník s matricí do nůžek ALC na DIN lišty, podélný oválný otvor 12x6,4mm","1ks",139.17187169466806,{"$f":"F148*(1-Elteq!$F$10)","v":139.17187169466806},""]
["TECHNIK SPECIAL - AKCIA","ALC/PR 12x6,4",null,"03006 ALFRA razník s matricí do nůžek ALC na DIN lišty, příčný oválný otvor 12x6,4mm","1ks",139.17187169466806,{"$f":"F149*(1-Elteq!$F$10)","v":139.17187169466806},""]
["TECHNIK SPECIAL - AKCIA","ALC-02",null,"03004 ALFRA pákové nůžky na DIN lišty TS 35x7,5 / 35x15 / 15x5,5 / Cu 10x3mm","1ks",1574.312212610085,{"$f":"F150*(1-Elteq!$F$10)","v":1574.312212610085},""]
["TECHNIK SPECIAL - AKCIA","ALC-H",null,"03003 ALFRA hydraulické nůžky s děrováním na DIN lišty TS 35x7,5/35x15/15x5,5/profil 34x15/Cu10x3mm","1ks",2442.3735669936277,{"$f":"F151*(1-Elteq!$F$10)","v":2442.3735669936277},""]
["TECHNIK SPECIAL - AKCIA","ALC-R1 AKCE",null,"03001 ALFRA pákové nůžky s děrováním 12x6,4 na DIN lišty 35x7,5/35x15/15x5,5/C-profil 34x15/Cu10x3mm","1ks",2103.9075750321949,{"$f":"F152*(1-Elteq!$F$10)","v":2103.9075750321949},""]
["TECHNIK SPECIAL - AKCIA","ALC-R2",null,"03002 ALFRA pákové nůžky s děrováním 5,5/6 na DIN lišty 35x7,5/35x15/15x5,5/C-profil 34x15/Cu 10x3mm","1ks",2103.9075750321949,{"$f":"F153*(1-Elteq!$F$10)","v":2103.9075750321949},""]
["TECHNIK SPECIAL - AKCIA","DUO",null,"03199 ALFRA pákové nůžky na DIN lišty TS 35x7,5 / 35x15mm","1ks",974.20310186267636,{"$f":"F154*(1-Elteq!$F$10)","v":974.20310186267636},""]
["TECHNIK SPECIAL - AKCIA","RC 300",null,"Pákové nůžky na DIN lišty TS 15x5,5 / 35x7,5 / 35x15mm","1ks",979.02772674809148,{"$f":"F155*(1-Elteq!$F$10)","v":979.02772674809148},"8591735012670"]
["TECHNIK SPECIAL - AKCIA","RC 500",null,"Pákové nůžky s děrováním na DIN lišty NS 35x7,5 / 35x15 / 15 a 32 a NLS-CU 3x10mm","1ks",1653.7329607238421,{"$f":"F156*(1-Elteq!$F$10)","v":1653.7329607238421},"8591735049768"]
["TECHNIK SPECIAL - AKCIA","RC 500 L65",null,"Děrovací razník k pákovým nůžkám RC500 pro otvor oválný 6,5x15mm","1ks",63.462373492768627,{"$f":"F157*(1-Elteq!$F$10)","v":63.462373492768627},"8591735049799"]
["TECHNIK SPECIAL - AKCIA","RC 500 R64",null,"Děrovací razník k pákovým nůžkám RC500 pro otvor kruhový 6,4mm","1ks",63.462373492768627,{"$f":"F158*(1-Elteq!$F$10)","v":63.462373492768627},"8591735049775"]
["TECHNIK SPECIAL - AKCIA","RC 500 R84",null,"Děrovací razník k pákovým nůžkám RC500 pro otvor kruhový 8,4mm","1ks",63.462373492768627,{"$f":"F159*(1-Elteq!$F$10)","v":63.462373492768627},"8591735049782"]
["TECHNIK SPECIAL - AKCIA","VKS 125",null,"03191 pákové nůžky na kabelové kanály do šíře 125mm (DC 125)","1ks",922.24560309666697,{"$f":"F160*(1-Elteq!$F$10)","v":922.24560309666697},"8591735013189"]
["TECHNIK SPECIAL - AKCIA","VKS 125 břit",null,"Náhradní břit k nůžkám VKS 125","1ks",127.66699696790882,{"$f":"F161*(1-Elteq!$F$10)","v":127.66699696790882},"8591735013196"]
["TECHNIK SPECIAL - AKCIA","VKS 125 džák",null,"Náhradní držák břitu k nůžkám VKS 125","1ks",25.60762439181892,{"$f":"F162*(1-Elteq!$F$10)","v":25.60762439181892},"8591735051884"]
["TECHNIK SPECIAL - AKCIA","LK330",null,"Elektronický popisovač bužírek L-MARK připojitelný k PC přes USB port, vč. kufru a SW pro Vista + XP","1ks",593.42886090606453,{"$f":"F163*(1-Elteq!$F$10)","v":593.42886090606453},"8591735040574"]
["TECHNIK SPECIAL - AKCIA","LK330 nůž",null,"Náhradní střihací nůž pro tiskárnu L-MARK model LK-330","1ks",18.185124568103291,{"$f":"F164*(1-Elteq!$F$10)","v":18.185124568103291},"8591735048662"]
["TECHNIK SPECIAL - AKCIA","M-1  Pro IV + kufr",null,"MK2500 elektronický popisovač bužírek CANON připojitelný k PC přes USB port, vč. kufru a SW","1ks",1302.6487190620928,{"$f":"F165*(1-Elteq!$F$10)","v":1302.6487190620928},"8591735046866"]
["TECHNIK SPECIAL - AKCIA","M-1  Std III + kufr",null,"MK1500 elektronický popisovač bužírek a samolepicích pásek CANON vč. kufru a příslušenství","1ks",749.67248219527858,{"$f":"F166*(1-Elteq!$F$10)","v":749.67248219527858},"8591735047016"]
["TECHNIK SPECIAL - AKCIA","M-1 adaptér 230V",null,"Síťový sdaptér 230V pro tiskárny bužírek CANON M-1","1ks",68.286998378183782,{"$f":"F167*(1-Elteq!$F$10)","v":68.286998378183782},"8591735040178"]
["TECHNIK SPECIAL - AKCIA","M-1 čistící sada",null,"3476A043 náhradní čistící sada pro navádění bužírky (molitanová vložka v plastovém dílu)","1ks",10.020374762016099,{"$f":"F168*(1-Elteq!$F$10)","v":10.020374762016099},"8591735020385"]
["TECHNIK SPECIAL - AKCIA","M-1 čistící sada 2",null,"3476A078 náhradní čistící sada pro navádění štítků (molitanová vložka v plastovém dílu)","1ks",29.875561790455407,{"$f":"F169*(1-Elteq!$F$10)","v":29.875561790455407},""]
["TECHNIK SPECIAL - AKCIA","M-1 čistící sada 3",null,"3476A071 náhradní čistící sada pro předehřívání bužírky (molitanová vložka v plastovém dílu)","1ks",39.339249065692833,{"$f":"F170*(1-Elteq!$F$10)","v":39.339249065692833},""]
["TECHNIK SPECIAL - AKCIA","M-1 deska OBM",null,"3471A032 vodící deska pro připojení obmotávací pásky","1ks",43.978311455515104,{"$f":"F171*(1-Elteq!$F$10)","v":43.978311455515104},""]
["TECHNIK SPECIAL - AKCIA","M-1 kufr AL",null,"4013B001 hliníkový kufr pro bezpečnou manipulaci a uložení tiskáren CANON M1","1ks",98.348122664232093,{"$f":"F172*(1-Elteq!$F$10)","v":98.348122664232093},""]
["TECHNIK SPECIAL - AKCIA","M-1 navádění",null,"3476A046 adaptér pro navádění bužírky","1ks",23.566436940297123,{"$f":"F173*(1-Elteq!$F$10)","v":23.566436940297123},"8591735020408"]
["TECHNIK SPECIAL - AKCIA","M-1 navádění 2",null,"3471A033 adaptér pro navádění pásku","1ks",172.75868339698127,{"$f":"F174*(1-Elteq!$F$10)","v":172.75868339698127},""]
["TECHNIK SPECIAL - AKCIA","M-1 nůž",null,"3476A042 náhradní dvoudílná sada nože pro přístroje M-1 (TM-CT03)","1sada",20.782999506403762,{"$f":"F175*(1-Elteq!$F$10)","v":20.782999506403762},"8591735020477"]
["TECHNIK SPECIAL - AKCIA","M-1 odvíjení",null,"Otočná podložka pro automatické a plynulé odvíjení bužírky z cívky","1ks",25.236499400633139,{"$f":"F176*(1-Elteq!$F$10)","v":25.236499400633139},"8591735051389"]
["TECHNIK SPECIAL - AKCIA","M-1 podávání",null,"3471A027 zařízení pro podávání bužírky v metráži pro tiskárny M-1","1ks",523.65736256313767,{"$f":"F177*(1-Elteq!$F$10)","v":523.65736256313767},""]
["TECHNIK SPECIAL - AKCIA","M-1 předehřívání",null,"3471A026 zařízení pro předehřívání bužírky v metráži pro tiskárny M-1","1ks",314.34286753435691,{"$f":"F178*(1-Elteq!$F$10)","v":314.34286753435691},"8591735047252"]
["TECHNIK SPECIAL - AKCIA","M-3E",null,"Elektrický potiskovač kabelů HOTMARKER, 7 znaků 2,4x2,4mm vč. transformátoru, pásky a kufru","1ks",2045.2698264248415,{"$f":"F179*(1-Elteq!$F$10)","v":2045.2698264248415},"8591735038717"]
["TECHNIK SPECIAL - AKCIA","M-3E razník",null,"Tiskové kolečko se znaky k tiskovým kleštím HOTMARKER M-3E","1ks",134.71837180043866,{"$f":"F180*(1-Elteq!$F$10)","v":134.71837180043866},"8591735038731"]
["TECHNIK SPECIAL - AKCIA","S700E",null,"Elektronický popisovač bužírek připojitelný k PC přes USB port, vč. kufru a SW pro Win7 + Vista + XP","1ks",593.42886090606453,{"$f":"F181*(1-Elteq!$F$10)","v":593.42886090606453},"8591735038021"]
["TECHNIK SPECIAL - AKCIA","TP76E",null,"Elektronický popisovač bužírek připojitelný k PC přes USB port, vč. kufru a SW","1ks",701.42623334112693,{"$f":"F182*(1-Elteq!$F$10)","v":701.42623334112693},""]
["TECHNIK SPECIAL - AKCIA","TP80E",null,"Elektronický popisovač bužírek připojitelný k PC přes USB port, vč. kufru a SW","1ks",798.28985604061597,{"$f":"F183*(1-Elteq!$F$10)","v":798.28985604061597},""]
["TECHNIK SPECIAL - AKCIA","SANITA 28,3 KPL",null,"01293 ALFRA prostřihovací čelisti průměr 28,3mm pro sanitární techniku, vč. šroubu M10x1","1sada",24.308686922668684,{"$f":"F184*(1-Elteq!$F$10)","v":24.308686922668684},""]
["TECHNIK SPECIAL - AKCIA","SANITA 28/32 KPL",null,"01456 ALFRA prostřihovací čelisti oboustranné 28/32mm pro sanitární techniku, vč. šroubu 10x55mm","1sada",42.864936481957756,{"$f":"F185*(1-Elteq!$F$10)","v":42.864936481957756},""]
["TECHNIK SPECIAL - AKCIA","SANITA 31,7 KPL",null,"01294 ALFRA prostřihovací čelisti průměr 31,7mm pro sanitární techniku, vč. šroubu M10x1","1sada",23.566436940297123,{"$f":"F186*(1-Elteq!$F$10)","v":23.566436940297123},""]
["TECHNIK SPECIAL - AKCIA","SANITA 35,0 KPL",null,"01295 ALFRA prostřihovací čelisti průměr 35,0mm pro sanitární techniku, vč. šroubu M10x1","1sada",28.576624321305172,{"$f":"F187*(1-Elteq!$F$10)","v":28.576624321305172},""]
["TECHNIK SPECIAL - AKCIA","SANITA SET",null,"01450 ALFRA sada prostřihovacích čelistí průměr 28,3/31,7/35,0mm pro sanitární techniku","1sada",97.049185195081847,{"$f":"F188*(1-Elteq!$F$10)","v":97.049185195081847},""]
["TECHNIK SPECIAL - AKCIA","SANITA ŠROUB 10x55",null,"01457 ALFRA náhradní šroub 10x55 speciál pro sanitární techniku","1ks",8.3503123016800824,{"$f":"F189*(1-Elteq!$F$10)","v":8.3503123016800824},""]
["TECHNIK SPECIAL - AKCIA","SANITA ŠROUB M10x1",null,"01299 ALFRA náhradní šroub M10x1 pro sanitární techniku","1ks",3.1545624250791424,{"$f":"F190*(1-Elteq!$F$10)","v":3.1545624250791424},""]
["TECHNIK SPECIAL - AKCIA","P 19,0x 19,0",null,"01302 ALFRA prostřihovací čelist - komplet vč. šroubu","1sada",175.17099583968886,{"$f":"F191*(1-Elteq!$F$10)","v":175.17099583968886},"8591735048778"]
["TECHNIK SPECIAL - AKCIA","P 22,0x 42,0",null,"01320 ALFRA prostřihovací čelist - komplet vč. šroubu","1sada",256.44736890937497,{"$f":"F192*(1-Elteq!$F$10)","v":256.44736890937497},"8591735049430"]
["TECHNIK SPECIAL - AKCIA","P 22,2x 22,2",null,"01303 ALFRA prostřihovací čelist - komplet vč. šroubu","1sada",185.19137060170496,{"$f":"F193*(1-Elteq!$F$10)","v":185.19137060170496},"8591735041403"]
["TECHNIK SPECIAL - AKCIA","P 25,4x 25,4",null,"01304 ALFRA prostřihovací čelist - komplet vč. šroubu","1sada",195.21174536372104,{"$f":"F194*(1-Elteq!$F$10)","v":195.21174536372104},""]
["TECHNIK SPECIAL - AKCIA","P 36,0x 52,0",null,"01325 ALFRA prostřihovací čelist - komplet vč. šroubu","1sada",582.29511117049105,{"$f":"F195*(1-Elteq!$F$10)","v":582.29511117049105},""]
["TECHNIK SPECIAL - AKCIA","P 36,0x 65,0",null,"01326 ALFRA prostřihovací čelist - komplet vč. šroubu","1sada",640.19060979547305,{"$f":"F196*(1-Elteq!$F$10)","v":640.19060979547305},""]
["TECHNIK SPECIAL - AKCIA","P 36,0x 86,0",null,"01327 ALFRA prostřihovací čelist - komplet vč. šroubu","1sada",719.24023291804451,{"$f":"F197*(1-Elteq!$F$10)","v":719.24023291804451},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK SPECIAL - AKCIA"},"P 45,0x 45,0",null,"Prostřihovací čelist - komplet vč. šroubu","1sada",510.66798787163526,{"$f":"F198*(1-Elteq!$F$10)","v":510.66798787163526},""]
["TECHNIK SPECIAL - AKCIA","P 45,0x 92,0",null,"01314 ALFRA prostřihovací čelist - komplet vč. šroubu pro hydraulické prostříhávání","1sada",782.70260641081313,{"$f":"F199*(1-Elteq!$F$10)","v":782.70260641081313},""]
["TECHNIK SPECIAL - AKCIA","P 45,5x 45,5",null,"01313 ALFRA prostřihovací čelist - komplet vč. šroubu pro hydraulické prostříhávání","1sada",504.35886302147702,{"$f":"F200*(1-Elteq!$F$10)","v":504.35886302147702},""]
["TECHNIK SPECIAL - AKCIA","P 46,0x 46,0",null,"01305 ALFRA prostřihovací čelist - komplet vč. šroubu pro hydraulické prostříhávání","1sada",490.62723834760311,{"$f":"F201*(1-Elteq!$F$10)","v":490.62723834760311},""]
["TECHNIK SPECIAL - AKCIA","P 46,0x 92,0",null,"01329 ALFRA prostřihovací čelist - komplet vč. šroubu pro hydraulické prostříhávání","1sada",781.21810644607001,{"$f":"F202*(1-Elteq!$F$10)","v":781.21810644607001},""]
["TECHNIK SPECIAL - AKCIA","P 68,0x 68,0",null,"01308 ALFRA prostřihovací čelist - komplet vč. šroubu pro hydraulické prostříhávání","1sada",695.48823348215444,{"$f":"F203*(1-Elteq!$F$10)","v":695.48823348215444},""]
["TECHNIK SPECIAL - AKCIA","P 68,0x 68,0 PLUS",null,"01315 ALFRA prostřihovací čelist pro nerez plech - komplet vč. šroubu pro hydraulické prostříhávání","1sada",1080.7159743329955,{"$f":"F204*(1-Elteq!$F$10)","v":1080.7159743329955},""]
["TECHNIK SPECIAL - AKCIA","P 68,0x138,0",null,"01330 ALFRA prostřihovací čelist - komplet vč. šroubu pro hydraulické prostříhávání","1sada",1068.4688496238648,{"$f":"F205*(1-Elteq!$F$10)","v":1068.4688496238648},""]
["TECHNIK SPECIAL - AKCIA","P 92,0x 92,0",null,"01309 ALFRA prostřihovací čelist - komplet vč. šroubu pro hydraulické prostříhávání","1sada",785.30048134911351,{"$f":"F206*(1-Elteq!$F$10)","v":785.30048134911351},""]
["TECHNIK SPECIAL - AKCIA","P125,0x125,0",null,"01431 ALFRA prostřihovací čelist - komplet vč. šroubu","1sada",1364.9977175813042,{"$f":"F207*(1-Elteq!$F$10)","v":1364.9977175813042},""]
["TECHNIK SPECIAL - AKCIA","STANDARD 12,7 KPL",null,"01001 ALFRA prostřihovací čelisti průměr 12,7mm Pg7 / M12 (matrice + razník + šroub 9,5x50)","1sada",25.60762439181892,{"$f":"F208*(1-Elteq!$F$10)","v":25.60762439181892},""]
["TECHNIK SPECIAL - AKCIA","STANDARD 16,2 KPL",null,"01009 ALFRA prostřihovací čelisti průměr 16,2mm M16 (matrice + razník + šroub 9,5x50)","1sada",22.081936975553997,{"$f":"F209*(1-Elteq!$F$10)","v":22.081936975553997},"8591735056773"]
["TECHNIK SPECIAL - AKCIA","STANDARD 20,4 KPL",null,"01033 ALFRA prostřihovací čelisti průměr 20,4mm M20 (matrice + razník + šroub 9,5x50)","1sada",22.824186957925559,{"$f":"F210*(1-Elteq!$F$10)","v":22.824186957925559},"8591735055172"]
["TECHNIK SPECIAL - AKCIA","STANDARD 22,5 KPL",null,"01045 ALFRA prostřihovací čelisti průměr 22,5mm Pg16 (matrice + razník + šroub 9,5x50)","1sada",23.751999435890014,{"$f":"F211*(1-Elteq!$F$10)","v":23.751999435890014},"8591735055189"]
["TECHNIK SPECIAL - AKCIA","STANDARD 25,4 KPL",null,"01057 ALFRA prostřihovací čelisti průměr 25,4mm M25 (matrice + razník + šroub 9,5x50)","1sada",30.061124286048297,{"$f":"F212*(1-Elteq!$F$10)","v":30.061124286048297},"8591735055165"]
["TECHNIK SPECIAL - AKCIA","STANDARD 28,3 KPL",null,"01069 ALFRA prostřihovací čelisti průměr 28,3mm Pg21 (matrice + razník + šroub 9,5x50)","1sada",27.83437433893361,{"$f":"F213*(1-Elteq!$F$10)","v":27.83437433893361},"8591735053079"]
["TECHNIK SPECIAL - AKCIA","STANDARD 30,5 KPL",null,"01093 ALFRA prostřihovací čelisti průměr 30,5mm (matrice + razník + šroub 9,5x50)","1sada",35.071311667056349,{"$f":"F214*(1-Elteq!$F$10)","v":35.071311667056349},""]
["TECHNIK SPECIAL - AKCIA","STANDARD 42,8 KPL",null,"01157 ALFRA prostřihovací čelisti průměr 42,8mm (matrice + razník + šroub 19x55)","1sada",64.575748466325976,{"$f":"F215*(1-Elteq!$F$10)","v":64.575748466325976},""]
["TECHNIK SPECIAL - AKCIA","STANDARD 65,0",null,"ALFRA prostřihovací čelisti průměr 65,0mm (matrice + razník) zakázková výroba","1pár",423.26805244738375,{"$f":"F216*(1-Elteq!$F$10)","v":423.26805244738375},""]
["TECHNIK SPECIAL - AKCIA","STANDARD 68,0 KPL",null,"01241 ALFRA prostřihovací čelisti průměr 68,0mm (matrice + razník + šroub 19x75)","1sada",152.1612463861704,{"$f":"F217*(1-Elteq!$F$10)","v":152.1612463861704},""]
["TECHNIK SPECIAL - AKCIA","STANDARD 70,0 KPL",null,"01221 ALFRA prostřihovací čelisti průměr 70,0mm (matrice + razník + šroub 19x75)","1sada",166.26399605123009,{"$f":"F218*(1-Elteq!$F$10)","v":166.26399605123009},""]
["TECHNIK SPECIAL - AKCIA","STANDARD 75,5 KPL",null,"01225 ALFRA prostřihovací čelisti průměr 75,5mm M75  (matrice + razník + šroub 19x75)","1sada",172.20199591020258,{"$f":"F219*(1-Elteq!$F$10)","v":172.20199591020258},""]
["TECHNIK SPECIAL - AKCIA","STANDARD 76,2 KPL",null,"01229 ALFRA prostřihovací čelisti průměr 76,2mm  (matrice + razník + šroub 19x75)","1sada",174.4287458573173,{"$f":"F220*(1-Elteq!$F$10)","v":174.4287458573173},""]
["TECHNIK SPECIAL - AKCIA","STANDARD 80,0 KPL",null,"01237 ALFRA prostřihovací čelisti průměr 80,0mm  (matrice + razník + šroub 19x75)","1sada",202.2631201962509,{"$f":"F221*(1-Elteq!$F$10)","v":202.2631201962509},""]
["TECHNIK SPECIAL - AKCIA","STANDARD 82,0 KPL",null,"01245 ALFRA prostřihovací čelisti průměr 82,0mm  (matrice + razník + šroub 19x75)","1sada",202.2631201962509,{"$f":"F222*(1-Elteq!$F$10)","v":202.2631201962509},""]
["TECHNIK SPECIAL - AKCIA","STANDARD 89,0",null,"01251+01252 ALFRA prostřihovací čelisti průměr 89,0mm (matrice + razník)","1pár",241.23124427075794,{"$f":"F223*(1-Elteq!$F$10)","v":241.23124427075794},""]
["TECHNIK SPECIAL - AKCIA","STANDARD 92,0",null,"01253+01254 ALFRA prostřihovací čelisti průměr 92,0mm (matrice + razník)","1pár",267.20999365376264,{"$f":"F224*(1-Elteq!$F$10)","v":267.20999365376264},""]
["TECHNIK SPECIAL - AKCIA","STANDARD SET Pg 7-48",null,"01297 ALFRA sada prostřihovacích čelistí Pg7 - Pg48 + 30,5mm STANDARD","1sada",470.95761381475666,{"$f":"F225*(1-Elteq!$F$10)","v":470.95761381475666},""]
["TECHNIK SPECIAL - AKCIA","STANDARD100,5",null,"01257+01258 ALFRA prostřihovací čelisti průměr 100,5mm (matrice + razník)","1pár",304.69361776352656,{"$f":"F226*(1-Elteq!$F$10)","v":304.69361776352656},""]
["TECHNIK SPECIAL - AKCIA","STANDARD120,0",null,"01267+01268 ALFRA prostřihovací čelisti průměr 120,0mm (matrice + razník)","1pár",371.86724116815304,{"$f":"F227*(1-Elteq!$F$10)","v":371.86724116815304},""]
["TECHNIK SPECIAL - AKCIA","ASN 15",null,"03016 ALFRA universální vysekávací nástroj 15,0 x 6,5mm","1ks",578.95498624981906,{"$f":"F228*(1-Elteq!$F$10)","v":578.95498624981906},""]
["TECHNIK SPECIAL - AKCIA","ASN 15 R",null,"03018 ALFRA náhradní razník do vysekávacího nástroje ASN 15","1ks",260.15861882123278,{"$f":"F229*(1-Elteq!$F$10)","v":260.15861882123278},""]
["TECHNIK SPECIAL - AKCIA","ASN 20",null,"03017 ALFRA universální vysekávací nástroj 20,0 x 9,0mm","1ks",587.86198603827779,{"$f":"F230*(1-Elteq!$F$10)","v":587.86198603827779},""]
["TECHNIK SPECIAL - AKCIA","ASN 20 R",null,"03019 ALFRA náhradní razník do vysekávacího nástroje ASN 20","1ks",293.26296803500452,{"$f":"F231*(1-Elteq!$F$10)","v":293.26296803500452},""]
["TECHNIK SPECIAL - AKCIA","ŠROUB  6x40",null,"01334 ALFRA šroub 6,0x40,0mm s kuličkovým ložiskem pro Tristar 12,5mm","1ks",7.7936248149014107,{"$f":"F232*(1-Elteq!$F$10)","v":7.7936248149014107},"8591735017910"]
["TECHNIK SPECIAL - AKCIA","ŠROUB  9,5x50",null,"01339 ALFRA šroub 9,5x50,0mm s kuličkovým ložiskem pro Tristar 15,2-30,5mm","1ks",7.7936248149014107,{"$f":"F233*(1-Elteq!$F$10)","v":7.7936248149014107},"8591735017927"]
["TECHNIK SPECIAL - AKCIA","ŠROUB 11,1x60",null,"01342 ALFRA šroub 11,1x60,0mm s kuličkovým ložiskem pro Tristar plus 15,2-25,4mm","1ks",23.751999435890014,{"$f":"F234*(1-Elteq!$F$10)","v":23.751999435890014},"8591735038892"]
["TECHNIK SPECIAL - AKCIA","ŠROUB 19x55",null,"01340 ALFRA šroub 19,0x55,0mm s kuličkovým ložiskem pro Tristar/Tristar plus 32,5-37,0mm","1ks",23.751999435890014,{"$f":"F235*(1-Elteq!$F$10)","v":23.751999435890014},"8591735017934"]
["TECHNIK SPECIAL - AKCIA","ŠROUB 19x75",null,"01341 ALFRA šroub 19,0x75,0mm s kuličkovým ložiskem pro Tristar/Tristar plus 40,5-63,5mm","1ks",27.83437433893361,{"$f":"F236*(1-Elteq!$F$10)","v":27.83437433893361},"8591735017941"]
["TECHNIK SPECIAL - AKCIA","ŠROUB BL  9,5x50",null,"01336 ALFRA šroub 9,5x50,0mm bez ložiska pro děrovací nástroje Tristar 15,2-30,5mm","1ks",1.8556249559289073,{"$f":"F237*(1-Elteq!$F$10)","v":1.8556249559289073},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 12,5",null,"01770 ALFRA prostřihovací čelisti do plechu M12 (matrice + razník)","1pár",28.205499330119391,{"$f":"F238*(1-Elteq!$F$10)","v":28.205499330119391},"4030266122648"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 12,5 KPL",null,"Prostřihovací čelisti M12 (matrice + razník + šroub 6,0x40) ALFRA","1sada",36.370249136206581,{"$f":"F239*(1-Elteq!$F$10)","v":36.370249136206581},"8591735050269"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 12,5 M",null,"01676 ALFRA prostřihovací čelisti do plechu M12 (matrice)","1ks",9.2781247796445356,{"$f":"F240*(1-Elteq!$F$10)","v":9.2781247796445356},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 12,5 R",null,"01675 ALFRA prostřihovací čelisti do plechu M12 (razník)","1ks",19.484062037253526,{"$f":"F241*(1-Elteq!$F$10)","v":19.484062037253526},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 15,2",null,"01771 ALFRA prostřihovací čelisti do plechu Pg 9 (matrice + razník)","1pár",29.318874303676736,{"$f":"F242*(1-Elteq!$F$10)","v":29.318874303676736},"4030266122662"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 15,2 KPL",null,"Prostřihovací čelisti Pg 9 (matrice + razník + šroub 9,5x50) ALFRA","1sada",37.854749100949711,{"$f":"F243*(1-Elteq!$F$10)","v":37.854749100949711},"8591735050207"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 15,2 M",null,"01682 ALFRA prostřihovací čelisti do plechu Pg 9 (matrice)","1ks",8.7214372928658648,{"$f":"F244*(1-Elteq!$F$10)","v":8.7214372928658648},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 15,2 R",null,"01681 ALFRA prostřihovací čelisti do plechu Pg 9 (razník)","1ks",23.009749453518449,{"$f":"F245*(1-Elteq!$F$10)","v":23.009749453518449},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 16,2",null,"01772 ALFRA prostřihovací čelisti do plechu M16 (matrice + razník)","1pár",30.988936764012752,{"$f":"F246*(1-Elteq!$F$10)","v":30.988936764012752},"4030266122679"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 16,2 KPL",null,"Prostřihovací čelisti M16 (matrice + razník + šroub 9,5x50) ALFRA","1sada",38.225874092135491,{"$f":"F247*(1-Elteq!$F$10)","v":38.225874092135491},"8591735050214"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 16,2 M",null,"01685 ALFRA prostřihovací čelisti do plechu M16 (matrice)","1ks",9.2781247796445356,{"$f":"F248*(1-Elteq!$F$10)","v":9.2781247796445356},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 16,2 R",null,"01684 ALFRA prostřihovací čelisti do plechu M16 (razník)","1ks",23.009749453518449,{"$f":"F249*(1-Elteq!$F$10)","v":23.009749453518449},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 18,6",null,"01773 ALFRA prostřihovací čelisti do plechu Pg 11 (matrice + razník)","1pár",31.360061755198533,{"$f":"F250*(1-Elteq!$F$10)","v":31.360061755198533},"4030266122686"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 18,6 KPL",null,"Prostřihovací čelisti Pg 11 (matrice + razník + šroub 9,5x50) ALFRA","1sada",38.225874092135491,{"$f":"F251*(1-Elteq!$F$10)","v":38.225874092135491},"8591735050221"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 18,6 M",null,"01688 ALFRA prostřihovací čelisti do plechu Pg 11 (matrice)","1ks",8.7214372928658648,{"$f":"F252*(1-Elteq!$F$10)","v":8.7214372928658648},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 18,6 R",null,"01687 ALFRA prostřihovací čelisti do plechu Pg 11 (razník)","1ks",23.009749453518449,{"$f":"F253*(1-Elteq!$F$10)","v":23.009749453518449},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 20,4",null,"01774 ALFRA prostřihovací čelisti Pg 13,5 / M20 (matrice + razník)","1pár",30.617811772826972,{"$f":"F254*(1-Elteq!$F$10)","v":30.617811772826972},"4030266122693"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 20,4 KPL",null,"Prostřihovací čelisti Pg 13,5 / M20 (matrice + razník + šroub 9,5x50) ALFRA","1sada",38.225874092135491,{"$f":"F255*(1-Elteq!$F$10)","v":38.225874092135491},"8591735034979"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 20,4 M",null,"01691 ALFRA prostřihovací čelisti Pg 13,5 / M20 (matrice)","1ks",8.7214372928658648,{"$f":"F256*(1-Elteq!$F$10)","v":8.7214372928658648},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 20,4 R",null,"01690 ALFRA prostřihovací čelisti Pg 13,5 / M20 (razník)","1ks",23.009749453518449,{"$f":"F257*(1-Elteq!$F$10)","v":23.009749453518449},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 22,5",null,"01775 ALFRA prostřihovací čelisti Pg 16 (matrice + razník)","1pár",32.658999224348769,{"$f":"F258*(1-Elteq!$F$10)","v":32.658999224348769},"4030266122709"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 22,5 KPL",null,"Prostřihovací čelisti Pg 16 (matrice + razník + šroub 9,5x50) ALFRA","1sada",40.452624039250182,{"$f":"F259*(1-Elteq!$F$10)","v":40.452624039250182},"8591735047573"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 22,5 M",null,"01694 ALFRA prostřihovací čelisti Pg 16 (matrice)","1ks",10.020374762016099,{"$f":"F260*(1-Elteq!$F$10)","v":10.020374762016099},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 22,5 R",null,"01693 ALFRA prostřihovací čelisti Pg 16 (razník)","1ks",24.308686922668684,{"$f":"F261*(1-Elteq!$F$10)","v":24.308686922668684},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK SPECIAL - AKCIA"},"TRISTAR 25,4",null,"01776 ALFRA prostřihovací čelisti M25 (matrice + razník)","1pár",37.854749100949711,{"$f":"F262*(1-Elteq!$F$10)","v":37.854749100949711},"4030266122747"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 25,4 KPL",null,"Prostřihovací čelisti M25 (matrice + razník + šroub 9,5x50) ALFRA","1sada",46.390623898222685,{"$f":"F263*(1-Elteq!$F$10)","v":46.390623898222685},"8591735047412"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 25,4 M",null,"01697 ALFRA prostřihovací čelisti M25 (matrice)","1ks",10.205937257608991,{"$f":"F264*(1-Elteq!$F$10)","v":10.205937257608991},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 25,4 R",null,"01696 ALFRA prostřihovací čelisti M25 (razník)","1ks",28.391061825712281,{"$f":"F265*(1-Elteq!$F$10)","v":28.391061825712281},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 28,3",null,"01777 ALFRA prostřihovací čelisti Pg 21 (matrice + razník)","1pár",35.813561649427911,{"$f":"F266*(1-Elteq!$F$10)","v":35.813561649427911},"4030266122716"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 28,3 KPL",null,"Prostřihovací čelisti Pg 21 (matrice + razník + šroub 9,5x50) ALFRA","1sada",43.792748959922214,{"$f":"F267*(1-Elteq!$F$10)","v":43.792748959922214},"8591735047405"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 28,3 M",null,"01700 ALFRA prostřihovací čelisti Pg 21 (matrice)","1ks",11.133749735573444,{"$f":"F268*(1-Elteq!$F$10)","v":11.133749735573444},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 28,3 R",null,"01699 ALFRA prostřihovací čelisti Pg 21 (razník)","1ks",25.79318688741181,{"$f":"F269*(1-Elteq!$F$10)","v":25.79318688741181},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 30,5",null,"01779 ALFRA prostřihovací čelisti 30,5mm (matrice + razník)","1pár",38.596999083321272,{"$f":"F270*(1-Elteq!$F$10)","v":38.596999083321272},"4030266122730"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 30,5 KPL",null,"Prostřihovací čelisti 30,5mm (matrice + razník + šroub 9,5x50) ALFRA","1sada",46.390623898222685,{"$f":"F271*(1-Elteq!$F$10)","v":46.390623898222685},"8591735050238"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 30,5 M",null,"01705 ALFRA prostřihovací čelisti 30,5mm (matrice)","1ks",12.061562213537897,{"$f":"F272*(1-Elteq!$F$10)","v":12.061562213537897},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 30,5 R",null,"01704 ALFRA prostřihovací čelisti 30,5mm (razník)","1ks",28.762186816898062,{"$f":"F273*(1-Elteq!$F$10)","v":28.762186816898062},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 32,5",null,"01780 ALFRA prostřihovací čelisti M32 (matrice + razník)","1pár",43.236061473143543,{"$f":"F274*(1-Elteq!$F$10)","v":43.236061473143543},"4030266125915"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 32,5 KPL",null,"Prostřihovací čelisti M32 (matrice + razník + šroub 19,0x55) ALFRA","1sada",67.730310891405111,{"$f":"F275*(1-Elteq!$F$10)","v":67.730310891405111},"8591735047429"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 32,5 M",null,"01710 ALFRA prostřihovací čelisti M32 (matrice)","1ks",15.958374620988602,{"$f":"F276*(1-Elteq!$F$10)","v":15.958374620988602},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 32,5 R",null,"01709 ALFRA prostřihovací čelisti M32 (razník)","1ks",29.133311808083846,{"$f":"F277*(1-Elteq!$F$10)","v":29.133311808083846},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 37,0",null,"01781 ALFRA prostřihovací čelisti Pg 29  (matrice + razník)","1pár",46.390623898222685,{"$f":"F278*(1-Elteq!$F$10)","v":46.390623898222685},"4030266122778"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 37,0 KPL",null,"Prostřihovací čelisti Pg 29  (matrice + razník + šroub 19,0x55) ALFRA","1sada",79.420748113757227,{"$f":"F279*(1-Elteq!$F$10)","v":79.420748113757227},"8591735050252"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 37,0 M",null,"01623 ALFRA prostřihovací čelisti Pg 29 (matrice)","1ks",15.958374620988602,{"$f":"F280*(1-Elteq!$F$10)","v":15.958374620988602},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 37,0 R",null,"01714 ALFRA prostřihovací čelisti Pg 29 (razník)","1ks",33.77237419790611,{"$f":"F281*(1-Elteq!$F$10)","v":33.77237419790611},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 40,5",null,"01782 ALFRA prostřihovací čelisti M40  (matrice + razník)","1pár",47.132873880594246,{"$f":"F282*(1-Elteq!$F$10)","v":47.132873880594246},"4030266122761"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 40,5 KPL",null,"Prostřihovací čelisti M40  (matrice + razník + šroub 19,0x75) ALFRA","1sada",78.307373140199886,{"$f":"F283*(1-Elteq!$F$10)","v":78.307373140199886},"8591735047399"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 40,5 M",null,"01717 ALFRA prostřihovací čelisti M40 (matrice)","1ks",17.81399957691751,{"$f":"F284*(1-Elteq!$F$10)","v":17.81399957691751},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 40,5 R",null,"01716 ALFRA prostřihovací čelisti M40 (razník)","1ks",32.102311737570098,{"$f":"F285*(1-Elteq!$F$10)","v":32.102311737570098},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 43,2",null,"01789 ALFRA prostřihovací čelisti 43,2mm (matrice + razník)","1pár",64.575748466325976,{"$f":"F286*(1-Elteq!$F$10)","v":64.575748466325976},"8591735054991"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 47,0",null,"01783 ALFRA prostřihovací čelisti Pg 36  (matrice + razník)","1pár",67.17362340462644,{"$f":"F287*(1-Elteq!$F$10)","v":67.17362340462644},"4030266122785"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 47,0 KPL",null,"Prostřihovací čelisti Pg 36 (matrice + razník + šroub 19,0x75) ALFRA","1sada",103.54387254083302,{"$f":"F288*(1-Elteq!$F$10)","v":103.54387254083302},"8591735036584"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 47,0 M",null,"01629 ALFRA prostřihovací čelisti Pg 36 (matrice)","1ks",25.42206189622603,{"$f":"F289*(1-Elteq!$F$10)","v":25.42206189622603},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 47,0 R",null,"01721 ALFRA prostřihovací čelisti Pg 36 (razník)","1ks",46.019498907036898,{"$f":"F290*(1-Elteq!$F$10)","v":46.019498907036898},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 50,5",null,"01784 ALFRA prostřihovací čelisti M50 (matrice + razník)","1pár",83.131998025615047,{"$f":"F291*(1-Elteq!$F$10)","v":83.131998025615047},"4030266122815"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 50,5 KPL",null,"Prostřihovací čelisti M50 (matrice + razník + šroub 19,0x75) ALFRA","1sada",116.53324723233538,{"$f":"F292*(1-Elteq!$F$10)","v":116.53324723233538},"8591735050245"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 50,5 M",null,"01738 ALFRA prostřihovací čelisti do plechu rozměr M50 (matrice)","1ks",29.318874303676736,{"$f":"F293*(1-Elteq!$F$10)","v":29.318874303676736},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 50,5 R",null,"01737 ALFRA prostřihovací čelisti do plechu rozměr M50 (razník)","1ks",54.926498695495653,{"$f":"F294*(1-Elteq!$F$10)","v":54.926498695495653},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 54,0",null,"01785 ALFRA prostřihovací čelisti do plechu rozměr Pg 42 (matrice + razník)","1pár",86.100997955101292,{"$f":"F295*(1-Elteq!$F$10)","v":86.100997955101292},"4030266122792"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 54,0 KPL",null,"Prostřihovací čelisti Pg 42 (matrice + razník + šroub 19,0x75) ALFRA","1sada",120.61562213537897,{"$f":"F296*(1-Elteq!$F$10)","v":120.61562213537897},"8591735050276"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 54,0 M",null,"01635 ALFRA prostřihovací čelisti do plechu rozměr Pg 42 (matrice)","1ks",32.473436728755878,{"$f":"F297*(1-Elteq!$F$10)","v":32.473436728755878},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 54,0 R",null,"01728 ALFRA prostřihovací čelisti do plechu rozměr Pg 42 (razník)","1ks",55.483186182274331,{"$f":"F298*(1-Elteq!$F$10)","v":55.483186182274331},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 60,0",null,"01786 ALFRA prostřihovací čelisti do plechu rozměr Pg 48 (matrice + razník)","1pár",89.441122875773331,{"$f":"F299*(1-Elteq!$F$10)","v":89.441122875773331},"4030266122808"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 60,0 KPL",null,"Prostřihovací čelisti Pg 48 (matrice + razník + šroub 19,0x75) ALFRA","1sada",125.44024702079413,{"$f":"F300*(1-Elteq!$F$10)","v":125.44024702079413},"8591735038748"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 60,0 M",null,"01638 ALFRA prostřihovací čelisti do plechu rozměr Pg 48 (matrice)","1ks",36.370249136206581,{"$f":"F301*(1-Elteq!$F$10)","v":36.370249136206581},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 60,0 R",null,"01730 ALFRA prostřihovací čelisti do plechu rozměr Pg 48 (razník)","1ks",56.039873669053001,{"$f":"F302*(1-Elteq!$F$10)","v":56.039873669053001},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 63,5",null,"01787 ALFRA prostřihovací čelisti do plechu rozměr M63 (matrice + razník)","1pár",103.9149975320188,{"$f":"F303*(1-Elteq!$F$10)","v":103.9149975320188},"4030266122822"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 63,5 KPL",null,"Prostřihovací čelisti M63 (matrice + razník + šroub 19,0x75) ALFRA","1sada",143.62537158889742,{"$f":"F304*(1-Elteq!$F$10)","v":143.62537158889742},"8591735050283"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 63,5 M",null,"01741 ALFRA prostřihovací čelisti do plechu rozměr M63 (matrice)","1ks",35.44243665824213,{"$f":"F305*(1-Elteq!$F$10)","v":35.44243665824213},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR 63,5 R",null,"01740 ALFRA prostřihovací čelisti do plechu rozměr M63 (razník)","1ks",64.761310961918866,{"$f":"F306*(1-Elteq!$F$10)","v":64.761310961918866},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR SET M12-40",null,"01754 ALFRA sada prostřihovacích čelistí do plechu rozměry M12 - M40","1sada",318.05411744621472,{"$f":"F307*(1-Elteq!$F$10)","v":318.05411744621472},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR SET M16-63",null,"01755 ALFRA sada prostřihovacích čelistí do plechu rozměry M16 - M63","1sada",558.5431117346011,{"$f":"F308*(1-Elteq!$F$10)","v":558.5431117346011},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR SET M16-63 L",null,"01757 ALFRA sada prostřihovacích čelistí do plechu rozměry M16 - M63 bez příslušenství","1sada",419.37124003993307,{"$f":"F309*(1-Elteq!$F$10)","v":419.37124003993307},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR SET Pg 9-21",null,"01750 ALFRA sada prostřihovacích čelistí do plechu rozměry Pg 9 - Pg 21 + 30,5mm","1sada",248.65374409447358,{"$f":"F310*(1-Elteq!$F$10)","v":248.65374409447358},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR SET Pg 9-48",null,"01751 ALFRA sada prostřihovacích čelistí do plechu rozměry Pg 9 - Pg 48 + 30,5mm","1sada",622.74773520974134,{"$f":"F311*(1-Elteq!$F$10)","v":622.74773520974134},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 15,2",null,"01600 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 9 (matrice + razník)","1pár",87.399935424251538,{"$f":"F312*(1-Elteq!$F$10)","v":87.399935424251538},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 15,2 M",null,"01602 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 9 (matrice)","1ks",25.236499400633139,{"$f":"F313*(1-Elteq!$F$10)","v":25.236499400633139},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 15,2 R",null,"01601 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 9 (razník)","1ks",62.348998519211285,{"$f":"F314*(1-Elteq!$F$10)","v":62.348998519211285},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 15,2KPL",null,"Prostřihovací čelisti pro nerez Pg 9 (matrice + razník + šroub 11,1x60) ALFRA","1sada",111.70862234692022,{"$f":"F315*(1-Elteq!$F$10)","v":111.70862234692022},"8591735050382"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 16,2",null,"01656 ALFRA prostřihovací čelisti pro nerez plech rozměr M16 (matrice + razník)","1pár",90.183372858144892,{"$f":"F316*(1-Elteq!$F$10)","v":90.183372858144892},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 16,2 M",null,"01658 ALFRA prostřihovací čelisti pro nerez plech rozměr M16 (matrice)","1ks",24.123124427075794,{"$f":"F317*(1-Elteq!$F$10)","v":24.123124427075794},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 16,2 R",null,"01657 ALFRA prostřihovací čelisti pro nerez plech rozměr M16 (razník)","1ks",66.802498413440659,{"$f":"F318*(1-Elteq!$F$10)","v":66.802498413440659},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 16,2KPL",null,"Prostřihovací čelisti pro nerez M16 (matrice + razník + šroub 11,1x60) ALFRA","1sada",115.41987225877803,{"$f":"F319*(1-Elteq!$F$10)","v":115.41987225877803},"8591735050399"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 18,6",null,"01603 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 11 (matrice + razník)","1pár",92.59568530085248,{"$f":"F320*(1-Elteq!$F$10)","v":92.59568530085248},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 18,6 M",null,"01605 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 11 (matrice)","1ks",26.720999365376265,{"$f":"F321*(1-Elteq!$F$10)","v":26.720999365376265},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 18,6 R",null,"01604 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 11 (razník)","1ks",64.946873457511757,{"$f":"F322*(1-Elteq!$F$10)","v":64.946873457511757},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 18,6KPL",null,"Prostřihovací čelisti pro nerez Pg 11 (matrice + razník + šroub 11,1x60) ALFRA","1sada",116.53324723233538,{"$f":"F323*(1-Elteq!$F$10)","v":116.53324723233538},"8591735050405"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 20,4",null,"01606 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 13,5/M20 (matrice + razník)","1pár",99.275935142196545,{"$f":"F324*(1-Elteq!$F$10)","v":99.275935142196545},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 20,4 M",null,"01608 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 13/M20 (matrice)","1ks",26.720999365376265,{"$f":"F325*(1-Elteq!$F$10)","v":26.720999365376265},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK SPECIAL - AKCIA"},"TRISTAR PLUS 20,4 R",null,"01607 Prostřihovací čelisti pro nerez plech rozměr Pg 13/M20 (razník)","1ks",73.111623263598943,{"$f":"F326*(1-Elteq!$F$10)","v":73.111623263598943},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 20,4KPL",null,"Prostřihovací čelisti pro nerez Pg 13,5/M20 (matrice + razník + šroub 11,1x60) ALFRA","1sada",122.47124709130789,{"$f":"F327*(1-Elteq!$F$10)","v":122.47124709130789},"8591735050412"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 22,5",null,"01609 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 16 (matrice + razník)","1pár",101.31712259371834,{"$f":"F328*(1-Elteq!$F$10)","v":101.31712259371834},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 22,5 M",null,"01611 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 16 (matrice)","1ks",27.64881184334072,{"$f":"F329*(1-Elteq!$F$10)","v":27.64881184334072},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 22,5 R",null,"01610 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 16 (razník)","1ks",74.96724821952786,{"$f":"F330*(1-Elteq!$F$10)","v":74.96724821952786},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 22,5KPL",null,"Prostřihovací čelisti pro nerez Pg 16 (matrice + razník + šroub 11,1x60) ALFRA","1sada",125.44024702079413,{"$f":"F331*(1-Elteq!$F$10)","v":125.44024702079413},"8591735050429"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 25,4",null,"01659 ALFRA prostřihovací čelisti pro nerez plech rozměr M25 (matrice + razník)","1pár",105.77062248794772,{"$f":"F332*(1-Elteq!$F$10)","v":105.77062248794772},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 25,4 M",null,"01661 ALFRA prostřihovací čelisti pro nerez plech rozměr M25 (matrice)","1ks",27.64881184334072,{"$f":"F333*(1-Elteq!$F$10)","v":27.64881184334072},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 25,4 R",null,"01660 ALFRA prostřihovací čelisti pro nerez plech rozměr M25 (razník)","1ks",72.369373281227382,{"$f":"F334*(1-Elteq!$F$10)","v":72.369373281227382},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 25,4KPL",null,"Prostřihovací čelisti pro nerez M25 (matrice + razník + šroub 11,1x60) ALFRA","1sada",132.1204968621382,{"$f":"F335*(1-Elteq!$F$10)","v":132.1204968621382},"8591735050436"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 28,3",null,"01612 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 21 (matrice + razník)","1pár",90.183372858144892,{"$f":"F336*(1-Elteq!$F$10)","v":90.183372858144892},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 28,3 M",null,"01614 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 21 (matrice)","1ks",11.504874726759224,{"$f":"F337*(1-Elteq!$F$10)","v":11.504874726759224},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 28,3 R",null,"01613 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 21 (razník)","1ks",81.647498060871925,{"$f":"F338*(1-Elteq!$F$10)","v":81.647498060871925},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 28,3KPL",null,"Prostřihovací čelisti pro nerez Pg 21 (matrice + razník + šroub 19,0x55) ALFRA","1sada",116.53324723233538,{"$f":"F339*(1-Elteq!$F$10)","v":116.53324723233538},"8591735050443"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 30,5",null,"01615 ALFRA prostřihovací čelisti pro nerez plech rozměr 30,5mm (matrice + razník)","1pár",98.533685159824984,{"$f":"F340*(1-Elteq!$F$10)","v":98.533685159824984},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 30,5 M",null,"01617 ALFRA prostřihovací čelisti pro nerez plech rozměr 30,5mm (matrice)","1ks",13.174937187095242,{"$f":"F341*(1-Elteq!$F$10)","v":13.174937187095242},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 30,5 R",null,"01616 ALFRA prostřihovací čelisti pro nerez plech rozměr 30,5mm (razník)","1ks",80.905248078500364,{"$f":"F342*(1-Elteq!$F$10)","v":80.905248078500364},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 30,5KPL",null,"Prostřihovací čelisti pro nerez 30,5mm (matrice + razník + šroub 19,0x55) ALFRA","1sada",121.72899710893631,{"$f":"F343*(1-Elteq!$F$10)","v":121.72899710893631},"8591735050306"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 32,5",null,"01662 ALFRA prostřihovací čelisti pro nerez plech rozměr M32 (matrice + razník)","1pár",107.62624744387662,{"$f":"F344*(1-Elteq!$F$10)","v":107.62624744387662},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 32,5 M",null,"01664 ALFRA prostřihovací čelisti pro nerez plech rozměr M32 (matrice)","1ks",25.79318688741181,{"$f":"F345*(1-Elteq!$F$10)","v":25.79318688741181},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 32,5 R",null,"01663 ALFRA prostřihovací čelisti pro nerez plech rozměr M32 (razník)","1ks",79.791873104943008,{"$f":"F346*(1-Elteq!$F$10)","v":79.791873104943008},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 32,5KPL",null,"Prostřihovací čelisti pro nerez M32 (matrice + razník + šroub 19,0x55) ALFRA","1sada",133.23387183569554,{"$f":"F347*(1-Elteq!$F$10)","v":133.23387183569554},"8591735050313"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 37,0",null,"01621 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 29 (matrice + razník)","1pár",109.85299739099131,{"$f":"F348*(1-Elteq!$F$10)","v":109.85299739099131},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 37,0 M",null,"01623 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 29 (matrice)","1ks",20.226312019625091,{"$f":"F349*(1-Elteq!$F$10)","v":20.226312019625091},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 37,0 R",null,"01622 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 29 (razník)","1ks",95.007997743560054,{"$f":"F350*(1-Elteq!$F$10)","v":95.007997743560054},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 37,0KPL",null,"Prostřihovací čelisti pro nerez Pg 29 (matrice + razník + šroub 19,0x55) ALFRA","1sada",136.57399675636756,{"$f":"F351*(1-Elteq!$F$10)","v":136.57399675636756},"8591735050320"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 40,5",null,"01665 ALFRA prostřihovací čelisti pro nerez plech rozměr M40 (matrice + razník)","1pár",116.90437222352116,{"$f":"F352*(1-Elteq!$F$10)","v":116.90437222352116},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 40,5 M",null,"01667 ALFRA prostřihovací čelisti pro nerez plech rozměr M40 (matrice)","1ks",18.370687063696181,{"$f":"F353*(1-Elteq!$F$10)","v":18.370687063696181},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 40,5 R",null,"01666 ALFRA prostřihovací čelisti pro nerez plech rozměr M40 (razník)","1ks",96.306935212710286,{"$f":"F354*(1-Elteq!$F$10)","v":96.306935212710286},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 40,5KPL",null,"Prostřihovací čelisti pro nerez M40 (matrice + razník + šroub 19,0x75) ALFRA","1sada",146.96549650956945,{"$f":"F355*(1-Elteq!$F$10)","v":146.96549650956945},"8591735050337"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 47,0",null,"01627 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 36 (matrice + razník)","1pár",143.9964965800832,{"$f":"F356*(1-Elteq!$F$10)","v":143.9964965800832},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 47,0 M",null,"01629 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 36 (matrice)","1ks",27.463249347747826,{"$f":"F357*(1-Elteq!$F$10)","v":27.463249347747826},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 47,0 R",null,"01628 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 36 (razník)","1ks",105.77062248794772,{"$f":"F358*(1-Elteq!$F$10)","v":105.77062248794772},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 47,0KPL",null,"Prostřihovací čelisti pro nerez Pg 36 (matrice + razník + šroub 19,0x75) ALFRA","1sada",173.31537088375995,{"$f":"F359*(1-Elteq!$F$10)","v":173.31537088375995},"8591735050450"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 50,5",null,"01668 ALFRA prostřihovací čelisti pro nerez plech rozměr M50 (matrice + razník)","1pár",146.59437151838367,{"$f":"F360*(1-Elteq!$F$10)","v":146.59437151838367},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 50,5KPL",null,"Prostřihovací čelisti pro nerez M50 (matrice + razník + šroub 19,0x75) ALFRA","1sada",177.02662079561776,{"$f":"F361*(1-Elteq!$F$10)","v":177.02662079561776},"8591735050344"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 54,0",null,"01633 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 42 (matrice + razník)","1pár",161.06824617462917,{"$f":"F362*(1-Elteq!$F$10)","v":161.06824617462917},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 54,0 M",null,"01635 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 42 (matrice)","1ks",36.741374127392362,{"$f":"F363*(1-Elteq!$F$10)","v":36.741374127392362},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 54,0 R",null,"01634 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 42 (razník)","1ks",120.61562213537897,{"$f":"F364*(1-Elteq!$F$10)","v":120.61562213537897},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 54,0KPL",null,"Prostřihovací čelisti pro nerez Pg 42 (matrice + razník + šroub 19,0x75) ALFRA","1sada",195.9539953460926,{"$f":"F365*(1-Elteq!$F$10)","v":195.9539953460926},"8591735050351"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 60,0",null,"01636 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 48 (matrice + razník)","1pár",183.70687063696181,{"$f":"F366*(1-Elteq!$F$10)","v":183.70687063696181},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 60,0 M",null,"01638 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 48 (matrice)","1ks",38.411436587728382,{"$f":"F367*(1-Elteq!$F$10)","v":38.411436587728382},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 60,0 R",null,"01637 ALFRA prostřihovací čelisti pro nerez plech rozměr Pg 48 (razník)","1ks",139.17187169466806,{"$f":"F368*(1-Elteq!$F$10)","v":139.17187169466806},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 60,0KPL",null,"Prostřihovací čelisti pro nerez Pg 48 (matrice + razník + šroub 19,0x75) ALFRA","1sada",218.22149481723949,{"$f":"F369*(1-Elteq!$F$10)","v":218.22149481723949},"8591735050368"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 63,5",null,"01671 ALFRA prostřihovací čelisti pro nerez plech rozměr M63 (matrice + razník)","1pár",182.22237067221869,{"$f":"F370*(1-Elteq!$F$10)","v":182.22237067221869},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 63,5KPL",null,"Prostřihovací čelisti pro nerez M63 (matrice + razník + šroub 19,0x75) ALFRA","1sada",210.79899499352388,{"$f":"F371*(1-Elteq!$F$10)","v":210.79899499352388},"8591735050375"]
["TECHNIK SPECIAL - AKCIA","TRISTAR SET+ M16-40",null,"01652 ALFRA sada prostřihovacích čelistí pro nerez plech rozměry M16 - M40","1sada",549.26498695495661,{"$f":"F372*(1-Elteq!$F$10)","v":549.26498695495661},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR SET+ M16-63",null,"01653 ALFRA sada prostřihovacích čelistí pro nerez plech rozměry M16 - M63","1sada",877.71060415437319,{"$f":"F373*(1-Elteq!$F$10)","v":877.71060415437319},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR SET+ Pg 9-21",null,"ALFRA sada prostřihovacích čelistí pro nerez plech rozměry Pg 9 - Pg 21","1sada",676.18973394049385,{"$f":"F374*(1-Elteq!$F$10)","v":676.18973394049385},""]
["TECHNIK SPECIAL - AKCIA","TRISTAR SET+ Pg 9-48",null,"ALFRA sada prostřihovacích čelistí pro nerez plech rozměry Pg 9 - Pg 48","1sada",1395.2444043629455,{"$f":"F375*(1-Elteq!$F$10)","v":1395.2444043629455},""]
["TECHNIK SPECIAL - AKCIA","02056 kufr",null,"02056 ALFRA kufr plastový prázdný bez pěnové výplně pro sadu 01752","1ks",65.689123439883318,{"$f":"F376*(1-Elteq!$F$10)","v":65.689123439883318},""]
["TECHNIK SPECIAL - AKCIA","02059 kufr",null,"02059 ALFRA kufr plastový prázdný bez pěnové výplně pro sadu 01309","1ks",42.864936481957756,{"$f":"F377*(1-Elteq!$F$10)","v":42.864936481957756},""]
["TECHNIK SPECIAL - AKCIA","02062 kufr",null,"02062 ALFRA kufr plastový prázdný bez pěnové výplně pro sadu 01751","1ks",54.369811208716982,{"$f":"F378*(1-Elteq!$F$10)","v":54.369811208716982},""]
["TECHNIK SPECIAL - AKCIA","AKKU 18,0 V",null,"02071 ALFRA náhradní akumulátor 18 V pro AKKU COMPACT","1ks",217.47924483486793,{"$f":"F379*(1-Elteq!$F$10)","v":217.47924483486793},""]
["TECHNIK SPECIAL - AKCIA","AKKU COMPACT",null,"02074 elektrohydraulický prostřihovací nástroj bateriový bez baterie, kufru a příslušenství","1ks",1484.3144022475331,{"$f":"F380*(1-Elteq!$F$10)","v":1484.3144022475331},"8591735051808"]
["TECHNIK SPECIAL - AKCIA","AKKU COMPACT SET",null,"02070 elektrohydraulický prostřihovací nástroj bateriový vč. kufru, nabíječky a 2ks baterie","1sada",1996.2813275883184,{"$f":"F381*(1-Elteq!$F$10)","v":1996.2813275883184},""]
["TECHNIK SPECIAL - AKCIA","B-FC 48N",null,"Elektrohydraulický prostřihovací přístroj akumulátoruvý vč. kufru, nabíječky a akumulátorů","1sada",1919.087329421676,{"$f":"F382*(1-Elteq!$F$10)","v":1919.087329421676},"8591735047931"]
["TECHNIK SPECIAL - AKCIA","B-FL 750",null,"Elektrohydraulický prostřihovací nástroj akumulátoruvý vč. kufru, nabíječky a akumulátorů","1sada",2220.8119472557164,{"$f":"F383*(1-Elteq!$F$10)","v":2220.8119472557164},"8591735047924"]
["TECHNIK SPECIAL - AKCIA","COMBI",null,"02055 ALFRA ruční hydraulický prostřihovací nástroj úhlový bez příslušenství","1ks",686.95235868488146,{"$f":"F384*(1-Elteq!$F$10)","v":686.95235868488146},""]
["TECHNIK SPECIAL - AKCIA","COMBI SET",null,"02050 ALFRA ruční hydraulický prostřihovací nástroj úhlový vč. kufru a příslušenství","1sada",745.59010729223496,{"$f":"F385*(1-Elteq!$F$10)","v":745.59010729223496},""]
["TECHNIK SPECIAL - AKCIA","COMBI SET M16-40",null,"01766 ALFRA ruční hydraulický prostřihovací nástroj úhlový vč. kufru s razníky M16 - M40","1sada",972.71860189793324,{"$f":"F386*(1-Elteq!$F$10)","v":972.71860189793324},""]
["TECHNIK SPECIAL - AKCIA","COMBI SET M16-63",null,"01759 ALFRA ruční hydraulický prostřihovací nástroj úhlový vč. kufru s razníky M16 - M63","1sada",1146.4050977728789,{"$f":"F387*(1-Elteq!$F$10)","v":1146.4050977728789},""]
["TECHNIK SPECIAL - AKCIA","COMBI SET Pg9-48",null,"01753 ALFRA ruční hydraulický prostřihovací nástroj úhlový vč. kufru s razníky Pg9 - Pg48","1sada",1201.3315964683745,{"$f":"F388*(1-Elteq!$F$10)","v":1201.3315964683745},""]
["TECHNIK SPECIAL - AKCIA","COMBI SET+ M16-40",null,"01643 ALFRA ruční hydraulický prostřihovací nástroj úhlový vč. kufru s razníky M16 - M40 pro nerez","1sada",1292.6283443000768,{"$f":"F389*(1-Elteq!$F$10)","v":1292.6283443000768},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK SPECIAL - AKCIA"},"COMBI SET+ M16-63",null,"01655 ALFRA ruční hydraulický prostřihovací nástroj úhlový vč. kufru s razníky M16 - M63 pro nerez","1sada",1631.4654612526954,{"$f":"F390*(1-Elteq!$F$10)","v":1631.4654612526954},""]
["TECHNIK SPECIAL - AKCIA","COMBI SET+ Pg9-42",null,"01651 ALFRA ruční hydraulický prostřihovací nástroj úhlový vč. kufru s razníky Pg9 - Pg42 pro nerez","1sada",1644.0837109530119,{"$f":"F391*(1-Elteq!$F$10)","v":1644.0837109530119},""]
["TECHNIK SPECIAL - AKCIA","COMBI STD Pg7-48",null,"02052 ALFRA ruční hydraulický prostřihovací nástroj úhlový vč. kufru s razníky Pg7 - Pg48 standard","1sada",1144.5494728169501,{"$f":"F392*(1-Elteq!$F$10)","v":1144.5494728169501},""]
["TECHNIK SPECIAL - AKCIA","COMPACT",null,"02005 ALFRA ruční hydraulický prostřihovací nástroj přímý bez příslušenství","1ks",526.99748748380966,{"$f":"F393*(1-Elteq!$F$10)","v":526.99748748380966},""]
["TECHNIK SPECIAL - AKCIA","COMPACT FLEX",null,"02066 ALFRA ruční hydraulický prostřihovací nástroj s flexi hadicí bez příslušenství","1ks",731.11623263598949,{"$f":"F394*(1-Elteq!$F$10)","v":731.11623263598949},""]
["TECHNIK SPECIAL - AKCIA","COMPACT FLEX SET",null,"02065 ALFRA ruční hydraulický prostřihovací nástroj s flexi hadicí vč. kufru","1sada",868.80360436591434,{"$f":"F395*(1-Elteq!$F$10)","v":868.80360436591434},""]
["TECHNIK SPECIAL - AKCIA","COMPACT kufr",null,"02001K ALFRA náhradní prázdný plastový kufr pro nástroje COMPACT nebo COMBI","1ks",72.926060768006053,{"$f":"F396*(1-Elteq!$F$10)","v":72.926060768006053},""]
["TECHNIK SPECIAL - AKCIA","COMPACT SET",null,"02001 ALFRA ruční hydraulický prostřihovací nástroj přímý vč. kufru a příslušenství","1sada",582.29511117049105,{"$f":"F397*(1-Elteq!$F$10)","v":582.29511117049105},""]
["TECHNIK SPECIAL - AKCIA","COMPACT SET M16-40",null,"01765 ALFRA ruční hydraulický prostřihovací nástroj přímý vč. kufru s razníky M16 - M40","1sada",805.71235586433158,{"$f":"F398*(1-Elteq!$F$10)","v":805.71235586433158},""]
["TECHNIK SPECIAL - AKCIA","COMPACT SET M16-63",null,"01758 ALFRA ruční hydraulický prostřihovací nástroj přímý vč. kufru s razníky M16 - M63","1sada",984.59460161587822,{"$f":"F399*(1-Elteq!$F$10)","v":984.59460161587822},""]
["TECHNIK SPECIAL - AKCIA","COMPACT SET Pg9-48",null,"01752 ALFRA ruční hydraulický prostřihovací nástroj přímý vč. kufru s razníky Pg9 - Pg48","1sada",1041.7478502584886,{"$f":"F400*(1-Elteq!$F$10)","v":1041.7478502584886},""]
["TECHNIK SPECIAL - AKCIA","COMPACT SET+ M16-40",null,"01642 ALFRA ruční hydraulický prostřihovací nástroj přímý vč. kufru s razníky M16 - M40 pro nerez","1sada",1113.7460985485302,{"$f":"F401*(1-Elteq!$F$10)","v":1113.7460985485302},""]
["TECHNIK SPECIAL - AKCIA","COMPACT SET+ M16-63",null,"01654 ALFRA ruční hydraulický prostřihovací nástroj přímý vč. kufru s razníky M16 - M63 pro nerez","1sada",1498.9738393993714,{"$f":"F402*(1-Elteq!$F$10)","v":1498.9738393993714},""]
["TECHNIK SPECIAL - AKCIA","COMPACT SET+ Pg9-42",null,"01650 ALFRA ruční hydraulický prostřihovací nástroj přímý vč. kufru s razníky Pg9 - Pg42 pro nerez","1sada",1498.9738393993714,{"$f":"F403*(1-Elteq!$F$10)","v":1498.9738393993714},""]
["TECHNIK SPECIAL - AKCIA","COMPACT STD Pg9-42",null,"02006 ALFRA ruční hydraulický prostřihovací nástroj přímý vč. kufru s razníky Pg9 - Pg42 standard","1sada",868.80360436591434,{"$f":"F404*(1-Elteq!$F$10)","v":868.80360436591434},""]
["TECHNIK SPECIAL - AKCIA","COMPACT těsnění",null,"0250600 ALFRA náhradní souprava těsnění pro nástroje COMPACT","1sada",43.978311455515104,{"$f":"F405*(1-Elteq!$F$10)","v":43.978311455515104},""]
["TECHNIK SPECIAL - AKCIA","GRAFITOVÁ PASTA",null,"33005 ALFRA grafitová pasta 120g pro ruční prostřihování plechu","1ks",14.288312160652586,{"$f":"F406*(1-Elteq!$F$10)","v":14.288312160652586},""]
["TECHNIK SPECIAL - AKCIA","HYDR. RED 19x40/9,5",null,"ALFRA hydraulický šroub 19,0 x 40mm pro TRISTAR (pouze redukce z 19mm na 9,5mm)","1ks",11.875999717945007,{"$f":"F407*(1-Elteq!$F$10)","v":11.875999717945007},"8591735055677"]
["TECHNIK SPECIAL - AKCIA","HYDR. RYCHLOSP. G1/4",null,"01453 ALFRA hydraulická rychlospojka G 1/4\" s vnitřním závitem (HR-M kolík CEJN)","1ks",30.803374268419862,{"$f":"F408*(1-Elteq!$F$10)","v":30.803374268419862},"8591735055684"]
["TECHNIK SPECIAL - AKCIA","HYDR. RYCHLOSP. R1/4",null,"01452 ALFRA hydraulická rychlospojka R 1/4\" s vnitřním závitem (HR-F objímka CEJN)","1ks",73.853873245970505,{"$f":"F409*(1-Elteq!$F$10)","v":73.853873245970505},"8591735055691"]
["TECHNIK SPECIAL - AKCIA","HYDR. ŠROUB  6",null,"02024 ALFRA hydraulický šroub 6,0 x 46mm pro TRISTAR (pouze šroub 6,0mm)","1ks",3.8968124074507053,{"$f":"F410*(1-Elteq!$F$10)","v":3.8968124074507053},"8591735055707"]
["TECHNIK SPECIAL - AKCIA","HYDR. ŠROUB  9,5",null,"02009 ALFRA hydraulický šroub 9,5 x 75mm pro TRISTAR (pouze šroub 9,5mm)","1ks",5.3813123721938307,{"$f":"F411*(1-Elteq!$F$10)","v":5.3813123721938307},"8591735055714"]
["TECHNIK SPECIAL - AKCIA","HYDR. ŠROUB 11,1",null,"01424 ALFRA hydraulický šroub 11,1 x 75mm pro TRISTAR PLUS (pouze šroub 11,1mm)","1ks",13.731624673873913,{"$f":"F412*(1-Elteq!$F$10)","v":13.731624673873913},"8591735055721"]
["TECHNIK SPECIAL - AKCIA","HYDR. ŠROUB 19",null,"02002 ALFRA hydraulický šroub 19,0mm pro TRISTAR a TRISTAR PLUS (stoupání 1,6mm)","1ks",23.195311949111343,{"$f":"F413*(1-Elteq!$F$10)","v":23.195311949111343},"8591735055738"]
["TECHNIK SPECIAL - AKCIA","HYDR. ŠROUB 19x 6",null,"02022 ALFRA hydraulický šroub 19,0 x 6,0mm pro TRISTAR (šroub 6,0mm vč. redukce 19mm)","1ks",15.216124638617039,{"$f":"F414*(1-Elteq!$F$10)","v":15.216124638617039},"8591735055745"]
["TECHNIK SPECIAL - AKCIA","HYDR. ŠROUB 19x 9,5",null,"02003 ALFRA hydraulický šroub 19,0 x 9,5mm pro TRISTAR (šroub 9,5mm vč. redukce 19mm)","1ks",17.62843708132462,{"$f":"F415*(1-Elteq!$F$10)","v":17.62843708132462},"8591735055752"]
["TECHNIK SPECIAL - AKCIA","HYDR. ŠROUB 19x 9,5P",null,"02010 ALFRA hydraulický šroub 19,0 x 9,5mm pro TRISTAR profesionální","1ks",78.678498131385666,{"$f":"F416*(1-Elteq!$F$10)","v":78.678498131385666},""]
["TECHNIK SPECIAL - AKCIA","HYDR. ŠROUB 19x11,1",null,"02007 ALFRA hydraulický šroub 19,0 x 11,1mm pro TRISTAR PLUS (šroub 11,1mm vč. redukce 19mm)","1ks",27.277686852154936,{"$f":"F417*(1-Elteq!$F$10)","v":27.277686852154936},"8591735055769"]
["TECHNIK SPECIAL - AKCIA","HYDR. ŠROUB 19x11,1P",null,"02011 ALFRA hydraulický šroub 19,0 x 11,1mm pro TRISTAR PLUS profesionální","1ks",78.678498131385666,{"$f":"F418*(1-Elteq!$F$10)","v":78.678498131385666},""]
["TECHNIK SPECIAL - AKCIA","HYDR. ŠROUBENÍ G1/4",null,"01454 ALFRA šroubení  G 1/4\" s vnějším závitem k hydraulickým rychlospojkám","1ks",12.432687204723679,{"$f":"F419*(1-Elteq!$F$10)","v":12.432687204723679},""]
["TECHNIK SPECIAL - AKCIA","KNZ 32/48",null,"03015 ALFRA pákové kleště na děrování zářezů proti pootočení (šířky zářezů 3,2mm a 4,8mm)","1ks",239.00449432364326,{"$f":"F420*(1-Elteq!$F$10)","v":239.00449432364326},"8591735037253"]
["TECHNIK SPECIAL - AKCIA","KNZ 32/48 razník",null,"030151 ALFRA náhradní razník do děrovacích kleští KNZ 32/48","1ks",125.9969345075728,{"$f":"F421*(1-Elteq!$F$10)","v":125.9969345075728},""]
["TECHNIK SPECIAL - AKCIA","LS6 Pg9-21",null,"BAUDAT ruční hydraulický prostřihovací nástroj vč. kufru s razníky Pg9 - Pg21 + 30,5mm","1sada",632.76810997175744,{"$f":"F422*(1-Elteq!$F$10)","v":632.76810997175744},""]
["TECHNIK SPECIAL - AKCIA","M ovál 13,5x20",null,"03241 ALFRA prostřihovací čelisti k děrovacímu přístroji ovál 13,5x20,0mm (pouze matrice) do 12mm","1pár",218.59261980842527,{"$f":"F423*(1-Elteq!$F$10)","v":218.59261980842527},""]
["TECHNIK SPECIAL - AKCIA","MATRICE L  6,6",null,"03230 ALFRA prostřihovací čelisti k děrovacímu přístroji průměr 6,6mm (matrice) do síly 5mm","1ks",65.874685935476208,{"$f":"F424*(1-Elteq!$F$10)","v":65.874685935476208},""]
["TECHNIK SPECIAL - AKCIA","MATRICE L  9,0",null,"03231 ALFRA prostřihovací čelisti k děrovacímu přístroji průměr 9,0mm (matrice) do síly 6mm","1ks",65.874685935476208,{"$f":"F425*(1-Elteq!$F$10)","v":65.874685935476208},""]
["TECHNIK SPECIAL - AKCIA","MATRICE L  9,5",null,"03232 ALFRA prostřihovací čelisti k děrovacímu přístroji průměr 9,5mm (matrice) do síly 6mm","1ks",65.874685935476208,{"$f":"F426*(1-Elteq!$F$10)","v":65.874685935476208},""]
["TECHNIK SPECIAL - AKCIA","MATRICE L 11,0",null,"03233 ALFRA prostřihovací čelisti k děrovacímu přístroji průměr 11,0mm (matrice) do síly 12mm","1ks",65.874685935476208,{"$f":"F427*(1-Elteq!$F$10)","v":65.874685935476208},""]
["TECHNIK SPECIAL - AKCIA","MATRICE L 13,5",null,"03235 ALFRA prostřihovací čelisti k děrovacímu přístroji průměr 13,5mm (matrice) do síly 12mm","1ks",65.874685935476208,{"$f":"F428*(1-Elteq!$F$10)","v":65.874685935476208},""]
["TECHNIK SPECIAL - AKCIA","MATRICE L 17,5",null,"03237 ALFRA prostřihovací čelisti k děrovacímu přístroji průměr 17,5mm (matrice) do síly 12mm","1ks",65.874685935476208,{"$f":"F429*(1-Elteq!$F$10)","v":65.874685935476208},""]
["TECHNIK SPECIAL - AKCIA","MATRICE L 21,5",null,"03240 ALFRA prostřihovací čelisti k děrovacímu přístroji průměr 21,5mm (matrice) do síly 12mm","1ks",65.874685935476208,{"$f":"F430*(1-Elteq!$F$10)","v":65.874685935476208},""]
["TECHNIK SPECIAL - AKCIA","MATRICE S  9,0",null,"03216 ALFRA prostřihovací čelisti k děrovacímu přístroji průměr 9,0mm (matrice) do síly 5mm","1ks",65.874685935476208,{"$f":"F431*(1-Elteq!$F$10)","v":65.874685935476208},""]
["TECHNIK SPECIAL - AKCIA","MATRICE S 11,0",null,"03218 ALFRA prostřihovací čelisti k děrovacímu přístroji průměr 11,0mm (matrice) do síly 5mm","1ks",65.874685935476208,{"$f":"F432*(1-Elteq!$F$10)","v":65.874685935476208},""]
["TECHNIK SPECIAL - AKCIA","MATRICE S 13,5",null,"03220 ALFRA prostřihovací čelisti k děrovacímu přístroji průměr 13,5mm (matrice) do síly 5mm","1ks",65.874685935476208,{"$f":"F433*(1-Elteq!$F$10)","v":65.874685935476208},""]
["TECHNIK SPECIAL - AKCIA","MATRICE S 6,6",null,"03215 ALFRA prostřihovací čelisti k děrovacímu přístroji průměr 6,6mm (matrice) do síly 5mm","1ks",65.874685935476208,{"$f":"F434*(1-Elteq!$F$10)","v":65.874685935476208},""]
["TECHNIK SPECIAL - AKCIA","P 22,5/20,1",null,"01422 ALFRA prostřihovací čelist průměr 22,5mm se sraženými rohy na 20,1mm - komplet vč. šroubu","1sada",387.82561578914164,{"$f":"F435*(1-Elteq!$F$10)","v":387.82561578914164},""]
["TECHNIK SPECIAL - AKCIA","P 22,5/3",null,"01420 ALFRA prostřihovací čelist průměr 22,5mm se zámkovým otvorem 3mm - komplet vč. šroubu","1sada",239.37561931482904,{"$f":"F436*(1-Elteq!$F$10)","v":239.37561931482904},""]
["TECHNIK SPECIAL - AKCIA","PODLOŽKY 3",null,"02004 ALFRA náhradní distanční podložky 3ks k prostřihovačům COMPACT a COMBI","1sada",28.019936834526501,{"$f":"F437*(1-Elteq!$F$10)","v":28.019936834526501},"8591735042745"]
["TECHNIK SPECIAL - AKCIA","PODLOŽKY 5",null,"02014 ALFRA náhradní distanční podložky 5ks k prostřihovací hlavici SKP1","1sada",51.40081127923073,{"$f":"F438*(1-Elteq!$F$10)","v":51.40081127923073},"8591735037710"]
["TECHNIK SPECIAL - AKCIA","PP 80",null,"Hydraulická prostřihovací hlavice do plechu","1ks",242.71574423550106,{"$f":"F439*(1-Elteq!$F$10)","v":242.71574423550106},""]
["TECHNIK SPECIAL - AKCIA","PP 80K",null,"Hydraulická prostřihovací hlavice do plechu v kufru s příslušenstvím","1ks",365.18699132680894,{"$f":"F440*(1-Elteq!$F$10)","v":365.18699132680894},""]
["TECHNIK SPECIAL - AKCIA","R+M ovál  9,5x20",null,"03241 ALFRA prostřihovací čelisti k děrovacímu přístroji ovál 9,5x20,0mm (razník + matrice) do 12mm","1pár",418.07230257078282,{"$f":"F441*(1-Elteq!$F$10)","v":418.07230257078282},""]
["TECHNIK SPECIAL - AKCIA","R+M ovál 11,0x20",null,"03241 ALFRA prostřihovací čelisti k děrovacímu přístroji ovál 11,0x20,0mm (razník + matrice) do 12mm","1pár",418.07230257078282,{"$f":"F442*(1-Elteq!$F$10)","v":418.07230257078282},""]
["TECHNIK SPECIAL - AKCIA","R+M ovál 12,5x20",null,"03241 ALFRA prostřihovací čelisti k děrovacímu přístroji ovál 12,5x20,0mm (razník + matrice) do 12mm","1pár",418.07230257078282,{"$f":"F443*(1-Elteq!$F$10)","v":418.07230257078282},""]
["TECHNIK SPECIAL - AKCIA","R+M ovál 13,5x20",null,"03241 ALFRA prostřihovací čelisti k děrovacímu přístroji ovál 13,5x20,0mm (razník + matrice) do 12mm","1pár",418.07230257078282,{"$f":"F444*(1-Elteq!$F$10)","v":418.07230257078282},""]
["TECHNIK SPECIAL - AKCIA","RAZNÍK  6,6",null,"03204 ALFRA prostřihovací čelisti k děrovacímu přístroji průměr 6,6mm (razník) do síly 5mm","1ks",159.02705872310736,{"$f":"F445*(1-Elteq!$F$10)","v":159.02705872310736},""]
["TECHNIK SPECIAL - AKCIA","RAZNÍK  9,0",null,"03205 ALFRA prostřihovací čelisti k děrovacímu přístroji průměr 9,0mm (razník) do síly 6mm","1ks",159.02705872310736,{"$f":"F446*(1-Elteq!$F$10)","v":159.02705872310736},""]
["TECHNIK SPECIAL - AKCIA","RAZNÍK  9,5",null,"03206 ALFRA prostřihovací čelisti k děrovacímu přístroji průměr 9,5mm (razník) do síly 6mm","1ks",159.02705872310736,{"$f":"F447*(1-Elteq!$F$10)","v":159.02705872310736},""]
["TECHNIK SPECIAL - AKCIA","RAZNÍK 11,0",null,"03207 ALFRA prostřihovací čelisti k děrovacímu přístroji průměr 11,0mm (razník) do síly 12mm","1ks",159.02705872310736,{"$f":"F448*(1-Elteq!$F$10)","v":159.02705872310736},""]
["TECHNIK SPECIAL - AKCIA","RAZNÍK 13,5",null,"03209 ALFRA prostřihovací čelisti k děrovacímu přístroji průměr 13,5mm (razník) do síly 12mm","1ks",159.02705872310736,{"$f":"F449*(1-Elteq!$F$10)","v":159.02705872310736},""]
["TECHNIK SPECIAL - AKCIA","RAZNÍK 17,5",null,"03211 ALFRA prostřihovací čelisti k děrovacímu přístroji průměr 17,5mm (razník) do síly 12mm","1ks",127.85255946350171,{"$f":"F450*(1-Elteq!$F$10)","v":127.85255946350171},""]
["TECHNIK SPECIAL - AKCIA","RAZNÍK 21,5",null,"03214 ALFRA prostřihovací čelisti k děrovacímu přístroji průměr 21,5mm (razník) do síly 12mm","1ks",127.85255946350171,{"$f":"F451*(1-Elteq!$F$10)","v":127.85255946350171},""]
["TECHNIK SPECIAL - AKCIA","SKP 1",null,"02012 ALFRA hydraulická prostřihovací hlavice do plechu","1ks",391.16574070981363,{"$f":"F452*(1-Elteq!$F$10)","v":391.16574070981363},"8591735037727"]
["TECHNIK SPECIAL - AKCIA","SKP 1 EL",null,"02025 ALFRA hydraulická prostřihovací hlavice s pohonem","1ks",3358.1244827445435,{"$f":"F453*(1-Elteq!$F$10)","v":3358.1244827445435},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK SPECIAL - AKCIA"},"SKP 1 MINI",null,"02013 ALFRA hydraulická prostřihovací hlavice do plechu, mini","1ks",261.27199379479015,{"$f":"F454*(1-Elteq!$F$10)","v":261.27199379479015},""]
["TECHNIK SPECIAL - AKCIA","SKP 1 NO",null,"02120 ALFRA hydraulická prostřihovací hlavice s pohonem","1ks",1321.204968621382,{"$f":"F455*(1-Elteq!$F$10)","v":1321.204968621382},""]
["TECHNIK SPECIAL - AKCIA","SPÍNAČ NOŽNÍ",null,"03865 ALFRA nožní spínač s funkcemi START / STOP / VYPNOUT","1ks",638.52054733513705,{"$f":"F456*(1-Elteq!$F$10)","v":638.52054733513705},""]
["TECHNIK SPECIAL - AKCIA","VRTÁK 10,0",null,"08036 ALFRA vrták HSS průměr 10,0mm pro TRISTAR","1ks",6.8658123369369566,{"$f":"F457*(1-Elteq!$F$10)","v":6.8658123369369566},""]
["TECHNIK SPECIAL - AKCIA","VRTÁK 11,5",null,"08035 ALFRA vrták HSS průměr 11,5mm pro TRISTAR PLUS","1ks",9.4636872752374277,{"$f":"F458*(1-Elteq!$F$10)","v":9.4636872752374277},""]
["TECHNIK SPECIAL - AKCIA","AB 01",null,"Odizolovací přístroj elektropneumatický pro vodiče o průměru 3,5-11,9mm","1ks",5558.3389929894493,{"$f":"F459*(1-Elteq!$F$10)","v":5558.3389929894493},""]
["TECHNIK SPECIAL - AKCIA","AI 01",null,"Odizolovací přístroj elektrický pro vodiče o průřezu 0,05-6mm2","1ks",2102.0519500762662,{"$f":"F460*(1-Elteq!$F$10)","v":2102.0519500762662},""]
["TECHNIK SPECIAL - AKCIA","AI 02",null,"Odizolovací přístroj elektrický pro vodiče o průřezu 0,05-2,5mm2","1ks",2475.4036912091624,{"$f":"F461*(1-Elteq!$F$10)","v":2475.4036912091624},""]
["TECHNIK SPECIAL - AKCIA","AI 03",null,"Odizolovací přístroj elektrický pro vodiče o průřezu 0,5-6mm2","1ks",2369.0763812344358,{"$f":"F462*(1-Elteq!$F$10)","v":2369.0763812344358},""]
["TECHNIK SPECIAL - AKCIA","AI 04",null,"Odizolovací přístroj elektrický pro vodiče o průřezu 2,5-16mm2","1ks",2475.4036912091624,{"$f":"F463*(1-Elteq!$F$10)","v":2475.4036912091624},""]
["TECHNIK SPECIAL - AKCIA","CM 25 - KA 11",null,"Locator - pozicioner na soustružené kontakty pro lisovací přístroj CM 25","1ks",59.751123580910814,{"$f":"F464*(1-Elteq!$F$10)","v":59.751123580910814},""]
["TECHNIK SPECIAL - AKCIA","CM 25-3",null,"Lisovací přístroj na soustružené kontakty s digitálním nástavcem 0,14-6mm2","1ks",3911.2862821069507,{"$f":"F465*(1-Elteq!$F$10)","v":3911.2862821069507},""]
["TECHNIK SPECIAL - AKCIA","CM 25-3-0146",null,"Lisovací čelist na soustružené kontakty 0,14-6mm2 pro lisovací přístroj CM 25","1ks",864.35010447168497,{"$f":"F466*(1-Elteq!$F$10)","v":864.35010447168497},""]
["TECHNIK SPECIAL - AKCIA","CRIMPER-G",null,"Lisovací přístroj na dutinky v roli pro průřezy 0,5-2,5mm2","1ks",4579.3112662413578,{"$f":"F467*(1-Elteq!$F$10)","v":4579.3112662413578},""]
["TECHNIK SPECIAL - AKCIA","CRIMPER-L",null,"Lisovací přístroj na dutinky sypané pro průřezy 0,5-2,5mm2","1ks",5341.9731231281385,{"$f":"F468*(1-Elteq!$F$10)","v":5341.9731231281385},""]
["TECHNIK SPECIAL - AKCIA","CS 60",null,"Odizolovací přístroj elektrický pro vodiče o průřezu 0,08-6mm2","1ks",2479.8571911033919,{"$f":"F469*(1-Elteq!$F$10)","v":2479.8571911033919},""]
["TECHNIK SPECIAL - AKCIA","DR 30",null,"Odvíjecí zařízení s talířem o průměru 300mm pro střihací a odizolovací přístroje, profi","1ks",285.39511822186591,{"$f":"F470*(1-Elteq!$F$10)","v":285.39511822186591},""]
["TECHNIK SPECIAL - AKCIA","DR 50",null,"Odvíjecí zařízení s talířem o průměru 500mm pro střihací a odizolovací přístroje, profi","1ks",940.80185265595605,{"$f":"F471*(1-Elteq!$F$10)","v":940.80185265595605},""]
["TECHNIK SPECIAL - AKCIA","DRN 400",null,"Navíjecí zařízení, buben o průměru 400mm pro navíjení kabelů a vodičů","1ks",126.55362199435147,{"$f":"F472*(1-Elteq!$F$10)","v":126.55362199435147},"8591735049966"]
["TECHNIK SPECIAL - AKCIA","DRO 500",null,"Odvíjecí zařízení s talířem o průměru 500mm pro střihací a odizolovací přístroje","1ks",73.853873245970505,{"$f":"F473*(1-Elteq!$F$10)","v":73.853873245970505},"8591735049959"]
["TECHNIK SPECIAL - AKCIA","EC 65",null,"Lisovací přístroj na kabelové koncovky vč. nožního ovládání","1ks",2632.0184374895621,{"$f":"F474*(1-Elteq!$F$10)","v":2632.0184374895621},""]
["TECHNIK SPECIAL - AKCIA","EC PP",null,"Plastový pojistný spínač k EC 65","1ks",8.9069997884587551,{"$f":"F475*(1-Elteq!$F$10)","v":8.9069997884587551},""]
["TECHNIK SPECIAL - AKCIA","EC PP OI056",null,"Plastový pojistný spínač k EC 65 s ochranným krytem pro kabelová oka izolovaná 0,5-6mm2","1ks",23.937561931482904,{"$f":"F476*(1-Elteq!$F$10)","v":23.937561931482904},""]
["TECHNIK SPECIAL - AKCIA","EC PP SK0144",null,"Plastový pojistný spínač k EC 65 s ochranným krytem pro soustružené kontakty 0,14-4mm2","1ks",23.937561931482904,{"$f":"F477*(1-Elteq!$F$10)","v":23.937561931482904},""]
["TECHNIK SPECIAL - AKCIA","ECM 03-N",null,"Odizolovací a lisovací přístroj na izolované dutinky v roli, pro průřezy 0,5-2,5mm2 / délka 8mm","1ks",5812.5596119517095,{"$f":"F478*(1-Elteq!$F$10)","v":5812.5596119517095},""]
["TECHNIK SPECIAL - AKCIA","EP-D 0141",null,"Lisovací přístroj na dutinky pro průřezy 0,14-1mm2","1ks",816.10385561753344,{"$f":"F479*(1-Elteq!$F$10)","v":816.10385561753344},""]
["TECHNIK SPECIAL - AKCIA","EP-D 0525",null,"Lisovací přístroj na dutinky pro průřezy 0,5-2,5mm2 (EP11676)","1ks",735.19860753903311,{"$f":"F480*(1-Elteq!$F$10)","v":735.19860753903311},"8591735035952"]
["TECHNIK SPECIAL - AKCIA","EP-MAG",null,"Magnetický držák k zavěšení přístrojů EP-D (EP11677)","1ks",59.379998589725034,{"$f":"F481*(1-Elteq!$F$10)","v":59.379998589725034},"8591735035969"]
["TECHNIK SPECIAL - AKCIA","HC 20",null,"Lisovací přístroj na soustružené kontakty s výměnnými nástavci (přístroj+baterie+kufr bez nástavců)","1ks",1347.5548429955725,{"$f":"F482*(1-Elteq!$F$10)","v":1347.5548429955725},""]
["TECHNIK SPECIAL - AKCIA","HC 20/ 6 STD",null,"Výměnný nástavec na soustružené kontakty 0,14-6mm2 pro přístroj HC 20","1ks",915.56535325532286,{"$f":"F483*(1-Elteq!$F$10)","v":915.56535325532286},""]
["TECHNIK SPECIAL - AKCIA","JQ 6100",null,"Střihací přístroj na bužírky do šíře 100mm","1ks",2095.0005752437364,{"$f":"F484*(1-Elteq!$F$10)","v":2095.0005752437364},""]
["TECHNIK SPECIAL - AKCIA","LC 100",null,"Střihací přístroj na vodiče pro průřezy 0,8-10mm2","1ks",2596.7615633269129,{"$f":"F485*(1-Elteq!$F$10)","v":2596.7615633269129},""]
["TECHNIK SPECIAL - AKCIA","MC 25",null,"Automat na izolované dutinky v roli 0,25-2,5mm2 (v ceně sada pro průřezy 0,5-2,5mm2)","1ks",5008.7028810433067,{"$f":"F486*(1-Elteq!$F$10)","v":5008.7028810433067},""]
["TECHNIK SPECIAL - AKCIA","MC2 0100",null,"Sada k MC 25 pro průřezy 0,25-0,34","1ks",502.50323806554809,{"$f":"F487*(1-Elteq!$F$10)","v":502.50323806554809},""]
["TECHNIK SPECIAL - AKCIA","MS 24",null,"Měřicí stůl pro odvíjecí, měřicí a navíjecí zařízení, pro měření délky kabelů a vodičů (pouze stůl)","1ks",215.43805738334615,{"$f":"F488*(1-Elteq!$F$10)","v":215.43805738334615},"8591735049973"]
["TECHNIK SPECIAL - AKCIA","MSK 28",null,"Měřicí zařízení pro měření délky kabelů a vodičů o průměru 1-16mm, rychlost protahování max. 40m/min","1ks",340.13605442176873,{"$f":"F489*(1-Elteq!$F$10)","v":340.13605442176873},"8591735050108"]
["TECHNIK SPECIAL - AKCIA","NCPP-10",null,"Lisovací přístroj na kontakty v páse do 2,5mm2","1ks",1362.7709676341894,{"$f":"F490*(1-Elteq!$F$10)","v":1362.7709676341894},""]
["TECHNIK SPECIAL - AKCIA","NCPP-20",null,"Lisovací přístroj na kontakty v páse do 6,0mm2","1ks",1634.0633361909959,{"$f":"F491*(1-Elteq!$F$10)","v":1634.0633361909959},""]
["TECHNIK SPECIAL - AKCIA","TM-3000",null,"Elektropneumatický lis na kabelové koncovky v páse","1ks",2330.2938196555219,{"$f":"F492*(1-Elteq!$F$10)","v":2330.2938196555219},""]
["TECHNIK SPECIAL - AKCIA","TM-EVFJ1",null,"Aplikátor MECAL pro konektory v páse MO/MOC 1,5-68","1ks",1602.8888369313902,{"$f":"F493*(1-Elteq!$F$10)","v":1602.8888369313902},""]
["TECHNIK SPECIAL - AKCIA","UNICUT 8",null,"Elektrický střihací přístroj na AL a Cu vodiče do průměru 8mm (plný vodič do průřezu 2,5mm2)","1ks",5217.6462510809015,{"$f":"F494*(1-Elteq!$F$10)","v":5217.6462510809015},""]
["TECHNIK SPECIAL - AKCIA","ZDBX  1",null,"Střihací a odizolovací elektrický přístroj pro vodiče o průřezu 0,05-0,75mm2","1ks",2421.219442496038,{"$f":"F495*(1-Elteq!$F$10)","v":2421.219442496038},""]
["TECHNIK SPECIAL - AKCIA","ZDBX  3",null,"Střihací a odizolovací elektrický přístroj pro vodiče o průřezu 0,05-4,0mm2","1ks",4675.8037639496606,{"$f":"F496*(1-Elteq!$F$10)","v":4675.8037639496606},"8591735040024"]
["TECHNIK SPECIAL - AKCIA","ZDBX  4",null,"Střihací a odizolovací elektrický přístroj pro vodiče o průřezu 0,08-10mm2","1ks",4784.9145113582799,{"$f":"F497*(1-Elteq!$F$10)","v":4784.9145113582799},"8591735040031"]
["TECHNIK SPECIAL - AKCIA","ZDBX 11",null,"Střihací a odizolovací elektrický přístroj pro kabely a vodiče o průřezu 0,5-16mm2","1ks",7821.4591892403441,{"$f":"F498*(1-Elteq!$F$10)","v":7821.4591892403441},"8591735048433"]
["TECHNIK SPECIAL - AKCIA","ZDBX 15",null,"Střihací a odizolovací elektrický přístroj pro kabely a vodiče o průřezu 0,5-30mm2","1ks",12845.749319913453,{"$f":"F499*(1-Elteq!$F$10)","v":12845.749319913453},""]
["TECHNIK SPECIAL - AKCIA","ZDBX 16",null,"Střihací a odizolovací elektrický přístroj pro kabely a vodiče o průřezu 4,0-70mm2","1ks",19998.812400028204,{"$f":"F500*(1-Elteq!$F$10)","v":19998.812400028204},""]
["TECHNIK SPECIAL - AKCIA","ZDBX 20",null,"Odizolovací elektrický přístroj pro vodiče o průřezu 0,05-2,5mm2","1ks",1855.2538309377214,{"$f":"F501*(1-Elteq!$F$10)","v":1855.2538309377214},"8591735040017"]
["TECHNIK SPECIAL - AKCIA","PP 600-D 1025",null,"Lisovací hlavice CHP100-AE51 k přístroji PP600 na dutinky pro průřezy 10-25mm2","1ks",844.30935494765276,{"$f":"F502*(1-Elteq!$F$10)","v":844.30935494765276},"8591735054878"]
["TECHNIK SPECIAL - AKCIA","AC 25",null,"Pneumatický lisovací přístroj na dutinky pro průřezy 0,25-2,5mm2, ruční model","1ks",270.92124356562044,{"$f":"F503*(1-Elteq!$F$10)","v":270.92124356562044},""]
["TECHNIK SPECIAL - AKCIA","AC 25 T",null,"Pneumatický lisovací přístroj na dutinky pro průřezy 0,25-2,5mm2, stolní model s pedálem","1ks",367.41374127392362,{"$f":"F504*(1-Elteq!$F$10)","v":367.41374127392362},""]
["TECHNIK SPECIAL - AKCIA","AC 40",null,"Pneumatický lisovací přístroj na dutinky pro průřezy 0,25-4,0mm2, ruční model","1ks",502.13211307436234,{"$f":"F505*(1-Elteq!$F$10)","v":502.13211307436234},""]
["TECHNIK SPECIAL - AKCIA","AC 40 T",null,"Pneumatický lisovací přístroj na dutinky pro průřezy 0,25-4,0mm2, stolní model","1ks",591.94436094132141,{"$f":"F506*(1-Elteq!$F$10)","v":591.94436094132141},""]
["TECHNIK SPECIAL - AKCIA","AC100",null,"Pneumatický lisovací přístroj na dutinky pro průřezy 4,0-10mm2, ruční model","1ks",360.73349143257957,{"$f":"F507*(1-Elteq!$F$10)","v":360.73349143257957},""]
["TECHNIK SPECIAL - AKCIA","AC100 T",null,"Pneumatický lisovací přístroj na dutinky pro průřezy 4,0-10mm2, stolní model","1ks",451.28798928191026,{"$f":"F508*(1-Elteq!$F$10)","v":451.28798928191026},""]
["TECHNIK SPECIAL - AKCIA","AC-DX",null,"Násuvný magnetický držák k pneumatickému lisovacímu přístroji AC25/AC100","1ks",24.865374409447359,{"$f":"F509*(1-Elteq!$F$10)","v":24.865374409447359},""]
["TECHNIK SPECIAL - AKCIA","AM 02",null,"Odizolovací a lisovací přístroj na dutinky izolované 0,5-2,5mm2 / 6, 8, 10, 12mm","1ks",14025.184541901866,{"$f":"F510*(1-Elteq!$F$10)","v":14025.184541901866},""]
["TECHNIK SPECIAL - AKCIA","AM 02 C",null,"Odizolovací a lisovací přístroj na dutinky izolované 0,14-0,34mm2 / 6-8mm","1ks",11415.062478892267,{"$f":"F511*(1-Elteq!$F$10)","v":11415.062478892267},""]
["TECHNIK SPECIAL - AKCIA","AM 02.1",null,"Odizolovací a lisovací přístroj na dutinky bez izolace 0,25-2,5mm2 / 6-12mm","1ks",15874.871497971802,{"$f":"F512*(1-Elteq!$F$10)","v":15874.871497971802},""]
["TECHNIK SPECIAL - AKCIA","AM 02-0,5/2,5",null,"Odizolovací a lisovací přístroj na dutinky izolované 0,5-2,5mm2 / 6, 8, 10mm","1ks",12185.146835602764,{"$f":"F513*(1-Elteq!$F$10)","v":12185.146835602764},""]
["TECHNIK SPECIAL - AKCIA","AM 04",null,"Odizolovací a lisovací přístroj na dutinky izolované 4-10mm2 / 10, 12, 18mm","1ks",17230.962215764648,{"$f":"F514*(1-Elteq!$F$10)","v":17230.962215764648},""]
["TECHNIK SPECIAL - AKCIA","BM-2A",null,"Stojan s držákem a svěrkou pro pneumatické lisovací přístroje WA22P a WA27F","1ks",141.76974663296852,{"$f":"F515*(1-Elteq!$F$10)","v":141.76974663296852},""]
["TECHNIK SPECIAL - AKCIA","MC  40L",null,"Automat na dutinky sypané 4,0-10mm2 (bez nástrojů)","1ks",7685.9985674575337,{"$f":"F516*(1-Elteq!$F$10)","v":7685.9985674575337},""]
["TECHNIK SPECIAL - AKCIA","MC  40L/ 4",null,"Lisovací nástroj k MC40L pro průřez 4,0mm2 / délka 10mm","1ks",1371.3068424314624,{"$f":"F517*(1-Elteq!$F$10)","v":1371.3068424314624},""]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK SPECIAL - AKCIA"},"MC  40L/ 6",null,"Lisovací nástroj k MC40L pro průřez 6,0mm2 / délka 12mm","1ks",1167.5592222704686,{"$f":"F518*(1-Elteq!$F$10)","v":1167.5592222704686},""]
["TECHNIK SPECIAL - AKCIA","MC  40L/10",null,"Lisovací nástroj k MC40L pro průřez 10mm2 / délka 12mm","1ks",1167.5592222704686,{"$f":"F519*(1-Elteq!$F$10)","v":1167.5592222704686},""]
["TECHNIK SPECIAL - AKCIA","MC 40",null,"Automat na izolované dutinky sypané 0,25-4,0 mm2 (v ceně sada pro průřezy 0,5-1,5mm2)","1ks",9029.4710355500629,{"$f":"F520*(1-Elteq!$F$10)","v":9029.4710355500629},""]
["TECHNIK SPECIAL - AKCIA","MC 40/258",null,"Lisovací nástroj k MC40 pro průřezy 2,5mm2 / délka 8mm","1ks",771.93998166642541,{"$f":"F521*(1-Elteq!$F$10)","v":771.93998166642541},""]
["TECHNIK SPECIAL - AKCIA","MC 40/346",null,"Lisovací nástroj k MC40 pro průřezy 0,25 a 0,34mm2 / délka 6mm","1ks",1042.8612252320459,{"$f":"F522*(1-Elteq!$F$10)","v":1042.8612252320459},""]
["TECHNIK SPECIAL - AKCIA","MC 40/348",null,"Lisovací nástroj k MC40 pro průřezy 0,25 a 0,34mm2 / délka 8mm","1ks",1042.8612252320459,{"$f":"F523*(1-Elteq!$F$10)","v":1042.8612252320459},""]
["TECHNIK SPECIAL - AKCIA","MC 40/410",null,"Lisovací nástroj k MC40 pro průřezy 4,0mm2 / délka 10mm","1ks",1232.1349707367945,{"$f":"F524*(1-Elteq!$F$10)","v":1232.1349707367945},""]
["TECHNIK SPECIAL - AKCIA","MC 40/L 6",null,"Rozšiřující sada k MC40 pro průřezy 0,5-1,5mm2 / délka 6mm","1ks",264.6121187154622,{"$f":"F525*(1-Elteq!$F$10)","v":264.6121187154622},""]
["TECHNIK SPECIAL - AKCIA","MC 40/L10",null,"Rozšiřující sada k MC40 pro průřezy 0,5-1,5mm2 / délka 10mm","1ks",264.6121187154622,{"$f":"F526*(1-Elteq!$F$10)","v":264.6121187154622},""]
["TECHNIK SPECIAL - AKCIA","MC 40/L12",null,"Rozšiřující sada k MC40 pro průřezy 0,5-1,5mm2 / délka 12mm","1ks",264.6121187154622,{"$f":"F527*(1-Elteq!$F$10)","v":264.6121187154622},""]
["TECHNIK SPECIAL - AKCIA","PP 600 adaptér",null,"Adaptér CP600/CSV10 pro výměnné čelisti typu C6 k pneumatickému lisovacímu přístroji PP600","1ks",339.20824194380424,{"$f":"F528*(1-Elteq!$F$10)","v":339.20824194380424},"8591735054670"]
["TECHNIK SPECIAL - AKCIA","PP 600 držák",null,"Souprava pro uchycení pneumatického přístroje PP600 ke stolu","1ks",321.02311737570096,{"$f":"F529*(1-Elteq!$F$10)","v":321.02311737570096},"8591735047894"]
["TECHNIK SPECIAL - AKCIA","PP 600 pedál",null,"Nožní ovládání k pneumatickému lisovacímu přístroji PP600","1ks",582.8517986572698,{"$f":"F530*(1-Elteq!$F$10)","v":582.8517986572698},"8591735047887"]
["TECHNIK SPECIAL - AKCIA","PP 600 tubus",null,"Pneumatický lisovací přístroj na koncovky pro průřezy 0,14-50mm2, pouze tubus CP600 !","1ks",1348.297092977944,{"$f":"F531*(1-Elteq!$F$10)","v":1348.297092977944},"8591735047863"]
["TECHNIK SPECIAL - AKCIA","PP 600-D 01410",null,"Lisovací hlavice CHP100-AE21 k přístroji PP600 na dutinky pro průřezy 0,14-10mm2","1ks",844.30935494765276,{"$f":"F532*(1-Elteq!$F$10)","v":844.30935494765276},"8591735054861"]
["TECHNIK SPECIAL - AKCIA","PP 600-MO 011",null,"Lisovací hlavice CHP100-F2,8 k přístroji PP600 na konektory bez izolace 2,8mm pro průřezy 0,1-1,0mm2","1ks",869.91697933947171,{"$f":"F533*(1-Elteq!$F$10)","v":869.91697933947171},"8591735054854"]
["TECHNIK SPECIAL - AKCIA","PP 600-MO 0525",null,"Lisovací hlavice CHP100-F4,8 k přístroji PP600 na konektory bez izolace 4,8mm pro průřezy 0,5-2,5mm2","1ks",869.91697933947171,{"$f":"F534*(1-Elteq!$F$10)","v":869.91697933947171},"8591735054847"]
["TECHNIK SPECIAL - AKCIA","PP 600-MO 056",null,"Lisovací hlavice CHP100-F6,3 k přístroji PP600 na konektory bez izolace 6,3mm pro průřezy 0,5-6mm2","1ks",869.91697933947171,{"$f":"F535*(1-Elteq!$F$10)","v":869.91697933947171},"8591735054830"]
["TECHNIK SPECIAL - AKCIA","PP 600-OI 056",null,"Lisovací hlavice CHP100-44 k přístroji PP600 na koncovky s izolací pro průřezy 0,5-6mm2","1ks",844.30935494765276,{"$f":"F536*(1-Elteq!$F$10)","v":844.30935494765276},"8591735054816"]
["TECHNIK SPECIAL - AKCIA","PP 600-OL 410",null,"Lisovací hlavice CHP100-RKS2 k přístroji PP600 na lehčená oka pro průřezy 4-10mm2","1ks",844.30935494765276,{"$f":"F537*(1-Elteq!$F$10)","v":844.30935494765276},"8591735047870"]
["TECHNIK SPECIAL - AKCIA","PP 600-ON 0110",null,"Lisovací hlavice CHP100-66 k přístroji PP600 na koncovky bez izolace pro průřezy 0,1-10mm2","1ks",844.30935494765276,{"$f":"F538*(1-Elteq!$F$10)","v":844.30935494765276},"8591735054823"]
["TECHNIK SPECIAL - AKCIA","UNIC-G",null,"Odizolovací a lisovací přístroj na dutinky v roli pro průřezy 0,5-2,5mm2 / délky 8mm","1ks",10202.968257679504,{"$f":"F539*(1-Elteq!$F$10)","v":10202.968257679504},""]
["TECHNIK SPECIAL - AKCIA","UNIC-L",null,"Odizolovací a lisovací přístroj na dutinky sypané pro průřezy 0,5-2,5mm2 / délky 8mm","1ks",10722.172120348412,{"$f":"F540*(1-Elteq!$F$10)","v":10722.172120348412},""]
["TECHNIK SPECIAL - AKCIA","UNIC-LS",null,"Odizolovací a lisovací přístroj na dutinky sypané pro průřezy 0,5-2,5mm2 / délky 6,8 a 10mm","1ks",13158.607687483067,{"$f":"F541*(1-Elteq!$F$10)","v":13158.607687483067},""]
["TECHNIK SPECIAL - AKCIA","UNIC-LZ",null,"Odizolovací a lisovací přístroj na dutinky dvojité sypané pro průřezy 2x0,5 - 2x1,5mm2","1ks",12671.320574056137,{"$f":"F542*(1-Elteq!$F$10)","v":12671.320574056137},""]
["TECHNIK SPECIAL - AKCIA","WA10A",null,"Nožní ovládání pro pneumatické lisovací přístroje WA22P a WA27F","1ks",155.13024631565665,{"$f":"F543*(1-Elteq!$F$10)","v":155.13024631565665},""]
["TECHNIK SPECIAL - AKCIA","WA22P",null,"Pneumatický lisovací přístroj na soustružené kontakty, průřez 0,34-1,5mm2","1ks",1601.7754619578327,{"$f":"F544*(1-Elteq!$F$10)","v":1601.7754619578327},""]
["TECHNIK SPECIAL - AKCIA","WA23",null,"Pneumatický lisovací přístroj na soustružené kontakty, průřez 6,0-16mm2","1ks",1875.8512679485325,{"$f":"F545*(1-Elteq!$F$10)","v":1875.8512679485325},""]
["TECHNIK SPECIAL - AKCIA","WA23-10",null,"Locator - pozicioner na soustružené kontakty, průřez 16mm2 pro pneumatický lis WA23","1ks",55.483186182274331,{"$f":"F546*(1-Elteq!$F$10)","v":55.483186182274331},""]
["TECHNIK SPECIAL - AKCIA","WA23-2",null,"Čelisti lisovací na soustružené kontakty, průřez 10mm2 pro pneumatický lis WA23","1ks",347.18742925429854,{"$f":"F547*(1-Elteq!$F$10)","v":347.18742925429854},""]
["TECHNIK SPECIAL - AKCIA","WA23-3",null,"Čelisti lisovací na soustružené kontakty, průřez 16mm2 pro pneumatický lis WA23","1ks",347.18742925429854,{"$f":"F548*(1-Elteq!$F$10)","v":347.18742925429854},""]
["TECHNIK SPECIAL - AKCIA","WA23-9",null,"Locator - pozicioner na soustružené kontakty, průřez 10mm2 pro pneumatický lis WA23","1ks",55.483186182274331,{"$f":"F549*(1-Elteq!$F$10)","v":55.483186182274331},""]
["TECHNIK SPECIAL - AKCIA","WA27F",null,"Pneumatický lisovací přístroj na soustružené kontakty, průřez 0,50-4,0mm2","1ks",1601.7754619578327,{"$f":"F550*(1-Elteq!$F$10)","v":1601.7754619578327},""]
["TECHNIK SPECIAL - AKCIA","18 ALU-60",null,"Čelisti na Al 70mm2 pro HP Z60","1pár",71.812685794448711,{"$f":"F551*(1-Elteq!$F$10)","v":71.812685794448711},"8591735042103"]
["TECHNIK SPECIAL - AKCIA","25 CU-60",null,"Čelisti na Cu DIN 185mm2, Al 150mm2 pro HP Z60","1pár",71.812685794448711,{"$f":"F552*(1-Elteq!$F$10)","v":71.812685794448711},"8591735042110"]
["TECHNIK SPECIAL - AKCIA","DRT  9,0",null,"Děrovací čelisti pro průměr 9,0mm k děrovací hlavici DP100Z plus","1pár",31.545624250791423,{"$f":"F553*(1-Elteq!$F$10)","v":31.545624250791423},"8591735046408"]
["TECHNIK SPECIAL - AKCIA","DRT 11,0",null,"Děrovací čelisti pro průměr 11,0mm k děrovací hlavici DP100Z plus","1pár",31.545624250791423,{"$f":"F554*(1-Elteq!$F$10)","v":31.545624250791423},"8591735047702"]
["TECHNIK SPECIAL - AKCIA","DRT 13,0",null,"Děrovací čelisti pro průměr 13,0mm k děrovací hlavici DP100Z plus","1pár",31.545624250791423,{"$f":"F555*(1-Elteq!$F$10)","v":31.545624250791423},"8591735054366"]
["TECHNIK SPECIAL - AKCIA","DRT 18,0",null,"Děrovací čelisti pro průměr 18,0mm k děrovací hlavici DP100Z plus","1pár",31.545624250791423,{"$f":"F556*(1-Elteq!$F$10)","v":31.545624250791423},"8591735056605"]
["TECHNIK SPECIAL - AKCIA","DRT 22x13",null,"Děrovací čelisti oválné pro otvor 22,0x13,0mm k děrovací hlavici DP100Z plus","1pár",81.461935565279035,{"$f":"F557*(1-Elteq!$F$10)","v":81.461935565279035},""]
["TECHNIK SPECIAL - AKCIA","RT  6,5",null,"Děrovací čelisti pro průměr 6,5mm k děrovací hlavici RHT160 a RHT160-60N","1pár",53.776011222819733,{"$f":"F558*(1-Elteq!$F$10)","v":53.776011222819733},"8591735039431"]
["TECHNIK SPECIAL - AKCIA","RT  7,0",null,"Děrovací čelisti pro průměr 7,0mm k děrovací hlavici RHT160 a RHT160-60N","1pár",53.776011222819733,{"$f":"F559*(1-Elteq!$F$10)","v":53.776011222819733},"8591735039318"]
["TECHNIK SPECIAL - AKCIA","RT  8,5",null,"Děrovací čelisti pro průměr 8,5mm k děrovací hlavici RHT160 a RHT160-60N","1pár",53.776011222819733,{"$f":"F560*(1-Elteq!$F$10)","v":53.776011222819733},"8591735039172"]
["TECHNIK SPECIAL - AKCIA","RT  9,0",null,"Děrovací čelisti pro průměr 9,0mm k děrovací hlavici RHT160 a RHT160-60N","1pár",53.776011222819733,{"$f":"F561*(1-Elteq!$F$10)","v":53.776011222819733},"8591735039417"]
["TECHNIK SPECIAL - AKCIA","RT 10,5",null,"Děrovací čelisti pro průměr 10,5mm k děrovací hlavici RHT160 a RHT160-60N","1pár",53.776011222819733,{"$f":"F562*(1-Elteq!$F$10)","v":53.776011222819733},"8591735039622"]
["TECHNIK SPECIAL - AKCIA","RT 11,0",null,"Děrovací čelisti pro průměr 11,0mm k děrovací hlavici RHT160 a RHT160-60N","1pár",53.776011222819733,{"$f":"F563*(1-Elteq!$F$10)","v":53.776011222819733},"8591735039202"]
["TECHNIK SPECIAL - AKCIA","RT 12,5",null,"Děrovací čelisti pro průměr 12,5mm k děrovací hlavici RHT160 a RHT160-60N","1pár",53.776011222819733,{"$f":"F564*(1-Elteq!$F$10)","v":53.776011222819733},"8591735039615"]
["TECHNIK SPECIAL - AKCIA","RT 13,0",null,"Děrovací čelisti pro průměr 13,0mm k děrovací hlavici RHT160 a RHT160-60N","1pár",53.776011222819733,{"$f":"F565*(1-Elteq!$F$10)","v":53.776011222819733},"8591735039189"]
["TECHNIK SPECIAL - AKCIA","RT 14,0",null,"Děrovací čelisti pro průměr 14,0mm k děrovací hlavici RHT160 a RHT160-60N","1pár",53.776011222819733,{"$f":"F566*(1-Elteq!$F$10)","v":53.776011222819733},"8591735039196"]
["TECHNIK SPECIAL - AKCIA","RT 14,5",null,"Děrovací čelisti pro průměr 14,5mm k děrovací hlavici RHT160 a RHT160-60N","1pár",53.776011222819733,{"$f":"F567*(1-Elteq!$F$10)","v":53.776011222819733},"8591735039158"]
["TECHNIK SPECIAL - AKCIA","RT 15,0",null,"Děrovací čelisti pro průměr 15,0mm k děrovací hlavici RHT160 a RHT160-60N","1pár",53.776011222819733,{"$f":"F568*(1-Elteq!$F$10)","v":53.776011222819733},"8591735039424"]
["TECHNIK SPECIAL - AKCIA","RT 17,0",null,"Děrovací čelisti pro průměr 17,0mm k děrovací hlavici RHT160 a RHT160-60N","1pár",53.776011222819733,{"$f":"F569*(1-Elteq!$F$10)","v":53.776011222819733},"8591735039080"]
["TECHNIK SPECIAL - AKCIA","A4-MO 2,8",null,"Locator k EC65 pro aretaci konektorů bez izolace šíře 2,8mm","1ks",55.668748677867221,{"$f":"F570*(1-Elteq!$F$10)","v":55.668748677867221},"8591735052164"]
["TECHNIK SPECIAL - AKCIA","A4-MO 4,8",null,"Locator k EC65 pro aretaci konektorů bez izolace šíře 4,8mm","1ks",55.668748677867221,{"$f":"F571*(1-Elteq!$F$10)","v":55.668748677867221},""]
["TECHNIK SPECIAL - AKCIA","A4-MO 6,3",null,"Locator k EC65 pro aretaci konektorů bez izolace šíře 6,3mm","1ks",55.668748677867221,{"$f":"F572*(1-Elteq!$F$10)","v":55.668748677867221},"8591735039066"]
["TECHNIK SPECIAL - AKCIA","C4-BP 0515B",null,"Čelisti k EC 65 na objímky s bočním připojením typ B, průřez 0,5-1,5mm2","1pár",222.3038697202831,{"$f":"F573*(1-Elteq!$F$10)","v":222.3038697202831},"8591735041977"]
["TECHNIK SPECIAL - AKCIA","C4-BP 0575",null,"Čelisti k EC 65 na objímky s bočním připojením, průřez 0,5-0,75mm2","1pár",153.64574635091353,{"$f":"F574*(1-Elteq!$F$10)","v":153.64574635091353},"8591735036249"]
["TECHNIK SPECIAL - AKCIA","C4-BP 115",null,"Čelisti k EC 65 na objímky s bočním připojením, průřez 1,0-1,5mm2","1pár",222.3038697202831,{"$f":"F575*(1-Elteq!$F$10)","v":222.3038697202831},"8591735035921"]
["TECHNIK SPECIAL - AKCIA","C4-BPI 1525",null,"Čelisti k EC 65 na izolované objímky s bočním připojením, průřez 1,5-2,5mm2","1pár",127.48143447231593,{"$f":"F576*(1-Elteq!$F$10)","v":127.48143447231593},"8591735036256"]
["TECHNIK SPECIAL - AKCIA","C4-D 0086",null,"Čelisti k EC 65 na dutinky, průřez 0,08-6mm2","1pár",101.50268508931123,{"$f":"F577*(1-Elteq!$F$10)","v":101.50268508931123},"8591735036263"]
["TECHNIK SPECIAL - AKCIA","C4-D 1025",null,"Čelisti k EC 65 na dutinky, průřez 10-25mm2","1pár",101.50268508931123,{"$f":"F578*(1-Elteq!$F$10)","v":101.50268508931123},"8591735036270"]
["TECHNIK SPECIAL - AKCIA","C4-D 3550",null,"Čelisti k EC 65 na dutinky, průřez 35-50mm2","1pár",174.61430835291017,{"$f":"F579*(1-Elteq!$F$10)","v":174.61430835291017},"8591735036287"]
["TECHNIK SPECIAL - AKCIA","C4-DD 410",null,"Čelisti k EC 65 na dutinky dvojité, průřez 4-10mm2","1pár",101.50268508931123,{"$f":"F580*(1-Elteq!$F$10)","v":101.50268508931123},"8591735036294"]
["TECHNIK SPECIAL - AKCIA","C4-MC3",null,"Čelisti k EC 65 na solární konektory MultiContact typ MC3","1pár",126.92474698553725,{"$f":"F581*(1-Elteq!$F$10)","v":126.92474698553725},"8591735042011"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK SPECIAL - AKCIA"},"C4-MO 0115",null,"EC R0115 lisovací čelisti k EC 65 na konektory bez izolace, průřez 0,14-1,5mm2","1pár",101.50268508931123,{"$f":"F582*(1-Elteq!$F$10)","v":101.50268508931123},"8591735036300"]
["TECHNIK SPECIAL - AKCIA","C4-MO 056",null,"Čelisti k EC 65 na konektory bez izolace, průřez 0,5-6mm2","1pár",101.50268508931123,{"$f":"F583*(1-Elteq!$F$10)","v":101.50268508931123},"8591735035938"]
["TECHNIK SPECIAL - AKCIA","C4-OI 0115",null,"Čelisti k EC 65 na oka izolovaná, průřez 0,10-1,5mm2","1pár",117.83218470148562,{"$f":"F584*(1-Elteq!$F$10)","v":117.83218470148562},"8591735039585"]
["TECHNIK SPECIAL - AKCIA","C4-OI 01425",null,"Čelisti k EC 65 na oka izolovaná NYLON, průřez 0,14-2,5mm2","1pár",156.98587127158555,{"$f":"F585*(1-Elteq!$F$10)","v":156.98587127158555},"8591735052980"]
["TECHNIK SPECIAL - AKCIA","C4-OI 02525",null,"Čelisti k EC 65 na oka izolovaná, průřez 0,25-2,5mm2","1pár",156.98587127158555,{"$f":"F586*(1-Elteq!$F$10)","v":156.98587127158555},"8591735042004"]
["TECHNIK SPECIAL - AKCIA","C4-OI 056",null,"Čelisti k EC 65 na oka izolovaná PVC, průřez 0,5-6mm2","1pár",82.575310538836376,{"$f":"F587*(1-Elteq!$F$10)","v":82.575310538836376},"8591735039578"]
["TECHNIK SPECIAL - AKCIA","C4-OI 056PA",null,"Čelisti k EC 65 na oka izolovaná PA, průřez 0,5-6mm2","1pár",140.65637165941118,{"$f":"F588*(1-Elteq!$F$10)","v":140.65637165941118},"8591735041991"]
["TECHNIK SPECIAL - AKCIA","C4-OI 056PC",null,"Čelisti k EC 65 na oka izolovaná PC, průřez 0,5-6mm2","1pár",140.65637165941118,{"$f":"F589*(1-Elteq!$F$10)","v":140.65637165941118},"8591735041984"]
["TECHNIK SPECIAL - AKCIA","C4-OL 03425",null,"Čelisti k EC 65 na oka lehčená, průřez 0,34-2,5mm2","1pár",82.575310538836376,{"$f":"F590*(1-Elteq!$F$10)","v":82.575310538836376},"8591735039592"]
["TECHNIK SPECIAL - AKCIA","C4-OL 410",null,"Čelisti k EC 65 na oka lehčená, průřez 4-10mm2","1pár",82.575310538836376,{"$f":"F591*(1-Elteq!$F$10)","v":82.575310538836376},"8591735039790"]
["TECHNIK SPECIAL - AKCIA","C4-ON 02525",null,"Čelisti k EC 65 na oka bez izolace, průřez 0,25-2,5mm2","1pár",82.575310538836376,{"$f":"F592*(1-Elteq!$F$10)","v":82.575310538836376},"8591735041960"]
["TECHNIK SPECIAL - AKCIA","C4-ON 0510",null,"Čelisti k EC 65 na oka bez izolace, průřez 0,5-10mm2","1pár",82.575310538836376,{"$f":"F593*(1-Elteq!$F$10)","v":82.575310538836376},"8591735035945"]
["TECHNIK SPECIAL - AKCIA","C4-ON 16",null,"Čelisti k EC 65 na oka bez izolace, průřez 16mm2","1pár",82.575310538836376,{"$f":"F594*(1-Elteq!$F$10)","v":82.575310538836376},"8591735039608"]
["TECHNIK SPECIAL - AKCIA","C4-SK 0144",null,"Čelisti k EC 65 na soustružené kontakty, průřez 0,14-4mm2","1pár",101.68824758490412,{"$f":"F595*(1-Elteq!$F$10)","v":101.68824758490412},"8591735039776"]
["TECHNIK SPECIAL - AKCIA","C4-SK 610",null,"Čelisti k EC 65 na soustružené kontakty, průřez 6-10mm2","1pár",156.98587127158555,{"$f":"F596*(1-Elteq!$F$10)","v":156.98587127158555},"8591735039783"]
["TECHNIK SPECIAL - AKCIA","10 CU-3D",null,"Čelisti lisovací na Cu DIN 25mm2, Al 10mm2 pro hydraulickou hlavici RH230, ECW-H3D","1pár",102.0593725760899,{"$f":"F597*(1-Elteq!$F$10)","v":102.0593725760899},"8591735038915"]
["TECHNIK SPECIAL - AKCIA","12 CU-3D",null,"Čelisti lisovací na Cu DIN 35mm2, Al 16-25mm2 pro hydraulickou hlavici RH230, ECW-H3D","1pár",102.0593725760899,{"$f":"F598*(1-Elteq!$F$10)","v":102.0593725760899},"8591735038922"]
["TECHNIK SPECIAL - AKCIA","14 CU-3D",null,"Čelisti lisovací na Cu DIN 50mm2, Al 35mm2 pro hydraulickou hlavici RH230, ECW-H3D","1pár",102.0593725760899,{"$f":"F599*(1-Elteq!$F$10)","v":102.0593725760899},"8591735038939"]
["TECHNIK SPECIAL - AKCIA","16 CU-3D",null,"Čelisti lisovací na Cu DIN 70mm2, Al 50mm2 pro hydraulickou hlavici RH230, ECW-H3D","1pár",102.0593725760899,{"$f":"F600*(1-Elteq!$F$10)","v":102.0593725760899},"8591735038946"]
["TECHNIK SPECIAL - AKCIA","18 CU-3D",null,"Čelisti lisovací na Cu DIN 95mm2, Al 70mm2 pro hydraulickou hlavici RH230, ECW-H3D","1pár",102.0593725760899,{"$f":"F601*(1-Elteq!$F$10)","v":102.0593725760899},"8591735038953"]
["TECHNIK SPECIAL - AKCIA","20 CU-3D",null,"Čelisti lisovací na Cu DIN 120mm2 pro hydraulickou hlavici RH230, ECW-H3D","1pár",102.0593725760899,{"$f":"F602*(1-Elteq!$F$10)","v":102.0593725760899},"8591735038960"]
["TECHNIK SPECIAL - AKCIA","22 CU-3D",null,"Čelisti lisovací na Cu DIN 150mm2, Al 95-120mm2 pro hydraulickou hlavici RH230, ECW-H3D","1pár",102.0593725760899,{"$f":"F603*(1-Elteq!$F$10)","v":102.0593725760899},"8591735038977"]
["TECHNIK SPECIAL - AKCIA","25 CU-3D",null,"Čelisti lisovací na Cu DIN 185mm2, Al 150mm2 pro hydraulickou hlavici RH230, ECW-H3D","1pár",102.0593725760899,{"$f":"F604*(1-Elteq!$F$10)","v":102.0593725760899},"8591735037369"]
["TECHNIK SPECIAL - AKCIA","28 CU-3D",null,"Čelisti lisovací na Cu DIN 240mm2, Al 185mm2 pro hydraulickou hlavici RH230, ECW-H3D","1pár",102.0593725760899,{"$f":"F605*(1-Elteq!$F$10)","v":102.0593725760899},"8591735037376"]
["TECHNIK SPECIAL - AKCIA","32 CU-3D",null,"Čelisti lisovací na Cu DIN 300mm2, Al 240mm2 pro hydraulickou hlavici RH230, ECW-H3D","1pár",102.0593725760899,{"$f":"F606*(1-Elteq!$F$10)","v":102.0593725760899},"8591735037383"]
["TECHNIK SPECIAL - AKCIA","34 CU-3D",null,"Čelisti lisovací na Al 300mm2 pro hydraulickou hlavici RH230, ECW-H3D","1pár",102.0593725760899,{"$f":"F607*(1-Elteq!$F$10)","v":102.0593725760899},"8591735037390"]
["TECHNIK SPECIAL - AKCIA","38 CU-3D",null,"Čelisti lisovací na Al a Cu DIN 400mm2 pro hydraulickou hlavici RH230, ECW-H3D","1pár",102.0593725760899,{"$f":"F608*(1-Elteq!$F$10)","v":102.0593725760899},"8591735037406"]
["TECHNIK SPECIAL - AKCIA","42 CU-3D",null,"Čelisti lisovací na Cu DIN 500mm2 pro hydraulickou hlavici RH230, ECW-H3D","1pár",102.0593725760899,{"$f":"F609*(1-Elteq!$F$10)","v":102.0593725760899},"8591735037413"]
["TECHNIK SPECIAL - AKCIA","44 CU-3D",null,"Čelisti lisovací na Cu DIN 625mm², Al 500mm² pro hydraulickou hlavici RH230, ECW-H3D","1pár",102.0593725760899,{"$f":"F610*(1-Elteq!$F$10)","v":102.0593725760899},"8591735037239"]
["TECHNIK SPECIAL - AKCIA","8 CU-3D",null,"Čelisti lisovací na Cu DIN 16mm2 pro hydraulickou hlavici RH230, ECW-H3D","1pár",102.0593725760899,{"$f":"F611*(1-Elteq!$F$10)","v":102.0593725760899},"8591735038984"]
["TECHNIK SPECIAL - AKCIA","AU 230-130 D",null,"Adaptér k ECW-H3D / RH 230 pro čelisti typ \"C\"","1pár",171.64530842342393,{"$f":"F612*(1-Elteq!$F$10)","v":171.64530842342393},"8591735039523"]
["TECHNIK SPECIAL - AKCIA","L150-3D",null,"Čelisti lisovací na Cu lehčené 150mm2 pro hydraulickou hlavici RH230, ECW-H3D","1pár",137.13068424314625,{"$f":"F613*(1-Elteq!$F$10)","v":137.13068424314625},"8591735038991"]
["TECHNIK SPECIAL - AKCIA","L185-3D",null,"Čelisti lisovací na Cu lehčené 185mm2 pro hydraulickou hlavici RH230, ECW-H3D","1pár",137.13068424314625,{"$f":"F614*(1-Elteq!$F$10)","v":137.13068424314625},"8591735039004"]
["TECHNIK SPECIAL - AKCIA","L240-3D",null,"Čelisti lisovací na Cu lehčené 240mm2 pro hydraulickou hlavici RH230, ECW-H3D","1pár",137.13068424314625,{"$f":"F615*(1-Elteq!$F$10)","v":137.13068424314625},"8591735039011"]
["TECHNIK SPECIAL - AKCIA","L300-3D",null,"Čelisti lisovací na Cu lehčené 300mm2 pro hydraulickou hlavici RH230, ECW-H3D","1pár",137.13068424314625,{"$f":"F616*(1-Elteq!$F$10)","v":137.13068424314625},"8591735039028"]
["TECHNIK SPECIAL - AKCIA","L400-3D",null,"Čelisti lisovací na Cu lehčené 400mm2 pro hydraulickou hlavici RH230, ECW-H3D","1pár",137.13068424314625,{"$f":"F617*(1-Elteq!$F$10)","v":137.13068424314625},"8591735039035"]
["TECHNIK SPECIAL - AKCIA","L500-3D",null,"Čelisti lisovací na Cu lehčené 500mm2 pro hydraulickou hlavici RH230, ECW-H3D","1pár",137.13068424314625,{"$f":"F618*(1-Elteq!$F$10)","v":137.13068424314625},"8591735039042"]
["TECHNIK SPECIAL - AKCIA","L625-3D",null,"Čelisti lisovací na Cu lehčené 625mm2 pro hydraulickou hlavici RH230, ECW-H3D","1pár",137.13068424314625,{"$f":"F619*(1-Elteq!$F$10)","v":137.13068424314625},"8591735039059"]
["TECHNIK SPECIAL - AKCIA","RU 120/95-3D",null,"Čelisti zkružovací na průřezy 120se / 95sm pro hydraulickou hlavici RH230, ECW-H3D","1pár",131.37824687976664,{"$f":"F620*(1-Elteq!$F$10)","v":131.37824687976664},"8591735054748"]
["TECHNIK SPECIAL - AKCIA","RU 150/120-3D",null,"Čelisti zkružovací na průřezy 150se /120sm pro hydraulickou hlavici RH230, ECW-H3D","1pár",131.37824687976664,{"$f":"F621*(1-Elteq!$F$10)","v":131.37824687976664},"8591735054755"]
["TECHNIK SPECIAL - AKCIA","RU 185/150-3D",null,"Čelisti zkružovací na průřezy 185se /150sm pro hydraulickou hlavici RH230, ECW-H3D","1pár",131.37824687976664,{"$f":"F622*(1-Elteq!$F$10)","v":131.37824687976664},"8591735054731"]
["TECHNIK SPECIAL - AKCIA","RU 240/185-3D",null,"Čelisti zkružovací na průřezy 240se /185sm pro hydraulickou hlavici RH230, ECW-H3D","1pár",131.37824687976664,{"$f":"F623*(1-Elteq!$F$10)","v":131.37824687976664},"8591735054762"]
["TECHNIK SPECIAL - AKCIA","RU 300/240-3D",null,"Čelisti zkružovací na průřezy 300se / 240sm pro hydraulickou hlavici RH230, ECW-H3D","1pár",131.37824687976664,{"$f":"F624*(1-Elteq!$F$10)","v":131.37824687976664},""]
["TECHNIK SPECIAL - AKCIA","C15-SK 014",null,"Čelisti na soustružené kontakty 0,1-4mm2 k EPG 15","1pár",140.84193415500405,{"$f":"F625*(1-Elteq!$F$10)","v":140.84193415500405},"8591735039233"]
["TECHNIK SPECIAL - AKCIA","10 ALU-22",null,"Čelisti na Al 10mm² pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F626*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025816"]
["TECHNIK SPECIAL - AKCIA","10 CU-22",null,"Čelisti na Cu DIN 25mm², Al 10mm² pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F627*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025823"]
["TECHNIK SPECIAL - AKCIA","12 ALU-22",null,"Čelisti na Al 16-25mm² pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F628*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025830"]
["TECHNIK SPECIAL - AKCIA","12 CU-22",null,"Čelisti na Cu DIN 35mm², Al 16-25mm² pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F629*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025847"]
["TECHNIK SPECIAL - AKCIA","14 ALU-22",null,"Čelisti na Al 35mm² pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F630*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025854"]
["TECHNIK SPECIAL - AKCIA","14 CU-22",null,"Čelisti na Cu DIN 50mm², Al 35mm² pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F631*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025861"]
["TECHNIK SPECIAL - AKCIA","16 ALU-22",null,"Čelisti na Al 50mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F632*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025878"]
["TECHNIK SPECIAL - AKCIA","16 CU-22",null,"Čelisti na Cu DIN 70mm2, Al 50mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F633*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025885"]
["TECHNIK SPECIAL - AKCIA","18 ALU-22",null,"Čelisti na Al 70mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F634*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025892"]
["TECHNIK SPECIAL - AKCIA","18 CU-22",null,"Čelisti na Cu DIN 95mm2, Al 70mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F635*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025908"]
["TECHNIK SPECIAL - AKCIA","20 CU-22",null,"Čelisti na Cu DIN 120mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F636*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025915"]
["TECHNIK SPECIAL - AKCIA","21 ALU-22",null,"Čelisti na AlFe110mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F637*(1-Elteq!$F$10)","v":48.431811349744478},"8591735039257"]
["TECHNIK SPECIAL - AKCIA","22 ALU-22",null,"Čelisti na Al 95-120mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F638*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025922"]
["TECHNIK SPECIAL - AKCIA","22 CU-22",null,"Čelisti na Cu DIN 150mm2, Al 95-120mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F639*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025939"]
["TECHNIK SPECIAL - AKCIA","25 ALU-22",null,"Čelisti na Al 150mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F640*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025946"]
["TECHNIK SPECIAL - AKCIA","25 CU-22",null,"Čelisti na Cu DIN 185mm2, Al 150mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F641*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025953"]
["TECHNIK SPECIAL - AKCIA","28 ALU-22",null,"Čelisti na Al 185mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F642*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025960"]
["TECHNIK SPECIAL - AKCIA","28 CU-22",null,"Čelisti na Cu DIN 240mm2, Al 185mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F643*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025977"]
["TECHNIK SPECIAL - AKCIA","32 ALU-22",null,"Čelisti na Al 240mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F644*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025984"]
["TECHNIK SPECIAL - AKCIA","34 ALU-22",null,"Čelisti na Al 300mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F645*(1-Elteq!$F$10)","v":48.431811349744478},"8591735029487"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK SPECIAL - AKCIA"},"5 CU-22",null,"Čelisti na Cu DIN 6mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F646*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025991"]
["TECHNIK SPECIAL - AKCIA","6 CU-22",null,"Čelisti na Cu DIN 10mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F647*(1-Elteq!$F$10)","v":48.431811349744478},"8591735026004"]
["TECHNIK SPECIAL - AKCIA","8 CU-22",null,"Čelisti na Cu DIN 16mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F648*(1-Elteq!$F$10)","v":48.431811349744478},"8591735026011"]
["TECHNIK SPECIAL - AKCIA","L  6-22",null,"Čelisti na Cu lehčené 6mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F649*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025687"]
["TECHNIK SPECIAL - AKCIA","L 10-22",null,"Čelisti na Cu lehčené 10mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F650*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025694"]
["TECHNIK SPECIAL - AKCIA","L 16-22",null,"Čelisti na Cu lehčené 16mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F651*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025700"]
["TECHNIK SPECIAL - AKCIA","L 25-22",null,"Čelisti na Cu lehčené 25mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F652*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025717"]
["TECHNIK SPECIAL - AKCIA","L 35-22",null,"Čelisti na Cu lehčené 35mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F653*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025724"]
["TECHNIK SPECIAL - AKCIA","L 50-22",null,"Čelisti na Cu lehčené 50mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F654*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025731"]
["TECHNIK SPECIAL - AKCIA","L 70-22",null,"Čelisti na Cu lehčené 70mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F655*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025748"]
["TECHNIK SPECIAL - AKCIA","L 95-22",null,"Čelisti na Cu lehčené 95mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F656*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025755"]
["TECHNIK SPECIAL - AKCIA","L120-22",null,"Čelisti na Cu lehčené 120mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F657*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025762"]
["TECHNIK SPECIAL - AKCIA","L150-22",null,"Čelisti na Cu lehčené 150mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F658*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025779"]
["TECHNIK SPECIAL - AKCIA","L185-22",null,"Čelisti na Cu lehčené 185mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F659*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025786"]
["TECHNIK SPECIAL - AKCIA","L240-22",null,"Čelisti na Cu lehčené 240mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F660*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025793"]
["TECHNIK SPECIAL - AKCIA","L300-22",null,"Čelisti na Cu lehčené 300mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",48.431811349744478,{"$f":"F661*(1-Elteq!$F$10)","v":48.431811349744478},"8591735025809"]
["TECHNIK SPECIAL - AKCIA","MO 16-22",null,"Oválné čelisti na průřez 25mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",76.785760676338185,{"$f":"F662*(1-Elteq!$F$10)","v":76.785760676338185},"8591735039394"]
["TECHNIK SPECIAL - AKCIA","MO 18-22",null,"Oválné čelisti na průřez 35mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",76.785760676338185,{"$f":"F663*(1-Elteq!$F$10)","v":76.785760676338185},"8591735039639"]
["TECHNIK SPECIAL - AKCIA","MO.12-22",null,"Oválné čelisti na průřez 16mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",76.785760676338185,{"$f":"F664*(1-Elteq!$F$10)","v":76.785760676338185},"8591735039240"]
["TECHNIK SPECIAL - AKCIA","MO.20-22",null,"Oválné čelisti na průřez 50mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",76.785760676338185,{"$f":"F665*(1-Elteq!$F$10)","v":76.785760676338185},"8591735039387"]
["TECHNIK SPECIAL - AKCIA","MO.22-22",null,"Oválné čelisti na průřez 70mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",76.785760676338185,{"$f":"F666*(1-Elteq!$F$10)","v":76.785760676338185},"8591735039653"]
["TECHNIK SPECIAL - AKCIA","MO.24-22",null,"Oválné čelisti na průřez 95mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",76.785760676338185,{"$f":"F667*(1-Elteq!$F$10)","v":76.785760676338185},"8591735039356"]
["TECHNIK SPECIAL - AKCIA","MO.26-22",null,"Oválné čelisti na průřez 120mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",76.785760676338185,{"$f":"F668*(1-Elteq!$F$10)","v":76.785760676338185},"8591735039646"]
["TECHNIK SPECIAL - AKCIA","PT 10-22",null,"Čelisti na dutinky 10mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",117.08993471911405,{"$f":"F669*(1-Elteq!$F$10)","v":117.08993471911405},"8591735054465"]
["TECHNIK SPECIAL - AKCIA","PT 16-22",null,"Čelisti na dutinky 16mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",117.08993471911405,{"$f":"F670*(1-Elteq!$F$10)","v":117.08993471911405},"8591735054458"]
["TECHNIK SPECIAL - AKCIA","PT 25-22",null,"Čelisti na dutinky 25mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",117.08993471911405,{"$f":"F671*(1-Elteq!$F$10)","v":117.08993471911405},"8591735054441"]
["TECHNIK SPECIAL - AKCIA","PT 35-22",null,"Čelisti na dutinky 35mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",117.08993471911405,{"$f":"F672*(1-Elteq!$F$10)","v":117.08993471911405},"8591735054434"]
["TECHNIK SPECIAL - AKCIA","PT 50-22",null,"Čelisti na dutinky 50mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",117.08993471911405,{"$f":"F673*(1-Elteq!$F$10)","v":117.08993471911405},"8591735054427"]
["TECHNIK SPECIAL - AKCIA","PT 70-22",null,"Čelisti na dutinky 70mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",117.08993471911405,{"$f":"F674*(1-Elteq!$F$10)","v":117.08993471911405},"8591735041892"]
["TECHNIK SPECIAL - AKCIA","PT 95-22",null,"Čelisti na dutinky 95mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",117.08993471911405,{"$f":"F675*(1-Elteq!$F$10)","v":117.08993471911405},"8591735041939"]
["TECHNIK SPECIAL - AKCIA","PT120-22",null,"Čelisti na dutinky 120mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",117.08993471911405,{"$f":"F676*(1-Elteq!$F$10)","v":117.08993471911405},"8591735035310"]
["TECHNIK SPECIAL - AKCIA","PT150-22",null,"Čelisti na dutinky 150mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",117.08993471911405,{"$f":"F677*(1-Elteq!$F$10)","v":117.08993471911405},"8591735035327"]
["TECHNIK SPECIAL - AKCIA","PT185-22",null,"Čelisti na dutinky 185mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",117.08993471911405,{"$f":"F678*(1-Elteq!$F$10)","v":117.08993471911405},"8591735035334"]
["TECHNIK SPECIAL - AKCIA","PT240-22",null,"Čelisti na dutinky 240mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",117.08993471911405,{"$f":"F679*(1-Elteq!$F$10)","v":117.08993471911405},"8591735054410"]
["TECHNIK SPECIAL - AKCIA","RU  10-22",null,"Čelisti zkružovací na průřezy 10mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",56.967686147017453,{"$f":"F680*(1-Elteq!$F$10)","v":56.967686147017453},"8591735039691"]
["TECHNIK SPECIAL - AKCIA","RU  16-22",null,"Čelisti zkružovací na průřezy 16mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",56.967686147017453,{"$f":"F681*(1-Elteq!$F$10)","v":56.967686147017453},"8591735039677"]
["TECHNIK SPECIAL - AKCIA","RU  35/25-22",null,"Čelisti zkružovací na průřezy 35/25mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",56.967686147017453,{"$f":"F682*(1-Elteq!$F$10)","v":56.967686147017453},"8591735035181"]
["TECHNIK SPECIAL - AKCIA","RU  50/35-22",null,"Čelisti zkružovací na průřezy 50/35mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",56.967686147017453,{"$f":"F683*(1-Elteq!$F$10)","v":56.967686147017453},"8591735035167"]
["TECHNIK SPECIAL - AKCIA","RU  70/50-22",null,"Čelisti zkružovací na průřezy 70/50mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",56.967686147017453,{"$f":"F684*(1-Elteq!$F$10)","v":56.967686147017453},"8591735035143"]
["TECHNIK SPECIAL - AKCIA","RU  95/70-22",null,"Čelisti zkružovací na průřezy 95/70mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",56.967686147017453,{"$f":"F685*(1-Elteq!$F$10)","v":56.967686147017453},"8591735035129"]
["TECHNIK SPECIAL - AKCIA","RU 120/95-22",null,"Čelisti zkružovací na průřezy 120/95mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",56.967686147017453,{"$f":"F686*(1-Elteq!$F$10)","v":56.967686147017453},"8591735035112"]
["TECHNIK SPECIAL - AKCIA","RU 150/120-22",null,"Čelisti zkružovací na průřezy 150/120mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",56.967686147017453,{"$f":"F687*(1-Elteq!$F$10)","v":56.967686147017453},"8591735035105"]
["TECHNIK SPECIAL - AKCIA","RU 185/150-22",null,"Čelisti zkružovací na průřezy 185/150mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",56.967686147017453,{"$f":"F688*(1-Elteq!$F$10)","v":56.967686147017453},"8591735035099"]
["TECHNIK SPECIAL - AKCIA","RU 240/185-22",null,"Čelisti zkružovací na průřezy 240/185mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",56.967686147017453,{"$f":"F689*(1-Elteq!$F$10)","v":56.967686147017453},"8591735035082"]
["TECHNIK SPECIAL - AKCIA","RU 300/240-22",null,"Čelisti zkružovací na průřezy 300/240mm2 pro K22, HP60CK, AP60CK, P60CK","1pár",56.967686147017453,{"$f":"F690*(1-Elteq!$F$10)","v":56.967686147017453},"8591735035075"]
["TECHNIK SPECIAL - AKCIA","10 C",null,"Čelisti na Cu DIN 25mm², Al 10mm² pro HT131, RH131, RHM132, B131, AP130","1pár",50.287436305673388,{"$f":"F691*(1-Elteq!$F$10)","v":50.287436305673388},"8591735022495"]
["TECHNIK SPECIAL - AKCIA","12 C",null,"Čelisti na Cu DIN 35mm², Al 16-25mm² pro HT131, RH131, RHM132, B131, AP130","1pár",50.287436305673388,{"$f":"F692*(1-Elteq!$F$10)","v":50.287436305673388},"8591735022501"]
["TECHNIK SPECIAL - AKCIA","14 C",null,"Čelisti na Cu DIN 50mm², Al 35mm² pro HT131, RH131, RHM132, B131, AP130","1pár",50.287436305673388,{"$f":"F693*(1-Elteq!$F$10)","v":50.287436305673388},"8591735022518"]
["TECHNIK SPECIAL - AKCIA","16 C",null,"Čelisti na Cu DIN 70mm2, Al 50mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",50.287436305673388,{"$f":"F694*(1-Elteq!$F$10)","v":50.287436305673388},"8591735022525"]
["TECHNIK SPECIAL - AKCIA","18 C",null,"Čelisti na Cu DIN 95mm2, Al 70mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",50.287436305673388,{"$f":"F695*(1-Elteq!$F$10)","v":50.287436305673388},"8591735022532"]
["TECHNIK SPECIAL - AKCIA","20 C",null,"Čelisti na Cu DIN 120mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",50.287436305673388,{"$f":"F696*(1-Elteq!$F$10)","v":50.287436305673388},"8591735022549"]
["TECHNIK SPECIAL - AKCIA","22 C",null,"Čelisti na Cu DIN 150mm2, Al 95-120mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",50.287436305673388,{"$f":"F697*(1-Elteq!$F$10)","v":50.287436305673388},"8591735022556"]
["TECHNIK SPECIAL - AKCIA","25 C",null,"Čelisti na Cu DIN 185mm2, Al 150mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",50.287436305673388,{"$f":"F698*(1-Elteq!$F$10)","v":50.287436305673388},"8591735022563"]
["TECHNIK SPECIAL - AKCIA","28 C",null,"Čelisti na Cu DIN 240mm2, Al 185mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",50.287436305673388,{"$f":"F699*(1-Elteq!$F$10)","v":50.287436305673388},"8591735022570"]
["TECHNIK SPECIAL - AKCIA","28 C-ALU",null,"Čelisti na Al 185mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",50.287436305673388,{"$f":"F700*(1-Elteq!$F$10)","v":50.287436305673388},"8591735022587"]
["TECHNIK SPECIAL - AKCIA","32 C",null,"Čelisti na Cu DIN 300mm2, Al 240mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",50.287436305673388,{"$f":"F701*(1-Elteq!$F$10)","v":50.287436305673388},"8591735022594"]
["TECHNIK SPECIAL - AKCIA","32 C-ALU",null,"Čelisti na Al 240mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",50.287436305673388,{"$f":"F702*(1-Elteq!$F$10)","v":50.287436305673388},"8591735022600"]
["TECHNIK SPECIAL - AKCIA","34 C-ALU",null,"Čelisti na Al 300mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",50.287436305673388,{"$f":"F703*(1-Elteq!$F$10)","v":50.287436305673388},"8591735022617"]
["TECHNIK SPECIAL - AKCIA","6 C",null,"Čelisti na Cu DIN 10mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",50.287436305673388,{"$f":"F704*(1-Elteq!$F$10)","v":50.287436305673388},"8591735022624"]
["TECHNIK SPECIAL - AKCIA","8 C",null,"Čelisti na Cu DIN 16mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",50.287436305673388,{"$f":"F705*(1-Elteq!$F$10)","v":50.287436305673388},"8591735022631"]
["TECHNIK SPECIAL - AKCIA","L 10-C",null,"Čelisti na Cu lehčené 10mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.776011222819733,{"$f":"F706*(1-Elteq!$F$10)","v":53.776011222819733},"8591735025588"]
["TECHNIK SPECIAL - AKCIA","L 16-C",null,"Čelisti na Cu lehčené 16mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.776011222819733,{"$f":"F707*(1-Elteq!$F$10)","v":53.776011222819733},"8591735025557"]
["TECHNIK SPECIAL - AKCIA","L 25-C",null,"Čelisti na Cu lehčené 25mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.776011222819733,{"$f":"F708*(1-Elteq!$F$10)","v":53.776011222819733},"8591735025564"]
["TECHNIK SPECIAL - AKCIA","L 35-C",null,"Čelisti na Cu lehčené 35mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.776011222819733,{"$f":"F709*(1-Elteq!$F$10)","v":53.776011222819733},"8591735025571"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK SPECIAL - AKCIA"},"L 50-C",null,"Čelisti na Cu lehčené 50mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.776011222819733,{"$f":"F710*(1-Elteq!$F$10)","v":53.776011222819733},"8591735025595"]
["TECHNIK SPECIAL - AKCIA","L 70-C",null,"Čelisti na Cu lehčené 70mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.776011222819733,{"$f":"F711*(1-Elteq!$F$10)","v":53.776011222819733},"8591735025601"]
["TECHNIK SPECIAL - AKCIA","L 95-C",null,"Čelisti na Cu lehčené 95mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.776011222819733,{"$f":"F712*(1-Elteq!$F$10)","v":53.776011222819733},"8591735025618"]
["TECHNIK SPECIAL - AKCIA","L120-C",null,"Čelisti na Cu lehčené 120mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.776011222819733,{"$f":"F713*(1-Elteq!$F$10)","v":53.776011222819733},"8591735025625"]
["TECHNIK SPECIAL - AKCIA","L150-C",null,"Čelisti na Cu lehčené 150mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.776011222819733,{"$f":"F714*(1-Elteq!$F$10)","v":53.776011222819733},"8591735025632"]
["TECHNIK SPECIAL - AKCIA","L185-C",null,"Čelisti na Cu lehčené 185mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.776011222819733,{"$f":"F715*(1-Elteq!$F$10)","v":53.776011222819733},"8591735025649"]
["TECHNIK SPECIAL - AKCIA","L240-C",null,"Čelisti na Cu lehčené 240mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.776011222819733,{"$f":"F716*(1-Elteq!$F$10)","v":53.776011222819733},"8591735025656"]
["TECHNIK SPECIAL - AKCIA","L300-C",null,"Čelisti na Cu lehčené 300mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.776011222819733,{"$f":"F717*(1-Elteq!$F$10)","v":53.776011222819733},"8591735025663"]
["TECHNIK SPECIAL - AKCIA","L400-C",null,"Čelisti na Cu lehčené 400mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.776011222819733,{"$f":"F718*(1-Elteq!$F$10)","v":53.776011222819733},"8591735025670"]
["TECHNIK SPECIAL - AKCIA","MA  2-C",null,"Matrice k HT131 pro Cu oka lehčená, průřez 10mm2","1ks",28.947749312490952,{"$f":"F719*(1-Elteq!$F$10)","v":28.947749312490952},"8591735039332"]
["TECHNIK SPECIAL - AKCIA","MA  3-C",null,"Matrice k HT131 pro Cu oka lehčená, průřez 16mm2","1ks",28.947749312490952,{"$f":"F720*(1-Elteq!$F$10)","v":28.947749312490952},"8591735039547"]
["TECHNIK SPECIAL - AKCIA","MA  5-C",null,"Matrice k HT131 pro Cu oka lehčená, průřez 25mm2","1ks",28.947749312490952,{"$f":"F721*(1-Elteq!$F$10)","v":28.947749312490952},"8591735039455"]
["TECHNIK SPECIAL - AKCIA","MA  7-C",null,"Matrice k HT131 pro Cu oka lehčená, průřez 35mm2","1ks",28.947749312490952,{"$f":"F722*(1-Elteq!$F$10)","v":28.947749312490952},"8591735039554"]
["TECHNIK SPECIAL - AKCIA","MA 10-C",null,"Matrice k HT131 pro Cu oka lehčená, průřez 50mm2","1ks",28.947749312490952,{"$f":"F723*(1-Elteq!$F$10)","v":28.947749312490952},"8591735039363"]
["TECHNIK SPECIAL - AKCIA","MA 14-C",null,"Matrice k HT131 pro Cu oka lehčená, průřez 70mm2","1ks",28.947749312490952,{"$f":"F724*(1-Elteq!$F$10)","v":28.947749312490952},"8591735039516"]
["TECHNIK SPECIAL - AKCIA","MA 19-C",null,"Matrice k HT131 pro Cu oka lehčená, průřez 95mm2","1ks",28.947749312490952,{"$f":"F725*(1-Elteq!$F$10)","v":28.947749312490952},"8591735039325"]
["TECHNIK SPECIAL - AKCIA","MA 24-C",null,"Matrice k HT131 pro Cu oka lehčená, průřez 120mm2","1ks",28.947749312490952,{"$f":"F726*(1-Elteq!$F$10)","v":28.947749312490952},"8591735039370"]
["TECHNIK SPECIAL - AKCIA","MA 30-C",null,"Matrice k HT131 pro Cu oka lehčená, průřez 150mm2","1ks",28.947749312490952,{"$f":"F727*(1-Elteq!$F$10)","v":28.947749312490952},"8591735039530"]
["TECHNIK SPECIAL - AKCIA","MA 37-C",null,"Matrice k HT131 pro Cu oka lehčená, průřez 185mm2","1ks",28.947749312490952,{"$f":"F728*(1-Elteq!$F$10)","v":28.947749312490952},"8591735039493"]
["TECHNIK SPECIAL - AKCIA","MA 48-C",null,"Matrice k HT131 pro Cu oka lehčená, průřez 240mm2","1ks",28.947749312490952,{"$f":"F729*(1-Elteq!$F$10)","v":28.947749312490952},"8591735039561"]
["TECHNIK SPECIAL - AKCIA","MA 60-C",null,"Matrice k HT131 pro Cu oka lehčená, průřez 300mm2","1ks",28.947749312490952,{"$f":"F730*(1-Elteq!$F$10)","v":28.947749312490952},"8591735039479"]
["TECHNIK SPECIAL - AKCIA","MW 10-C",null,"Matrice k HT131 pro Cu oka stáčená z plechu dle DIN 46234, průřez 10mm2","1ks",204.48987014336558,{"$f":"F731*(1-Elteq!$F$10)","v":204.48987014336558},"8591735048907"]
["TECHNIK SPECIAL - AKCIA","MW 16-C",null,"Matrice k HT131 pro Cu oka stáčená z plechu dle DIN 46234, průřez 16mm2","1ks",204.48987014336558,{"$f":"F732*(1-Elteq!$F$10)","v":204.48987014336558},"8591735048914"]
["TECHNIK SPECIAL - AKCIA","MW 25-C",null,"Matrice k HT131 pro Cu oka stáčená z plechu dle DIN 46234, průřez 25mm2","1ks",204.48987014336558,{"$f":"F733*(1-Elteq!$F$10)","v":204.48987014336558},"8591735039752"]
["TECHNIK SPECIAL - AKCIA","MW 35-C",null,"Matrice k HT131 pro Cu oka stáčená z plechu dle DIN 46234, průřez 35mm2","1ks",204.48987014336558,{"$f":"F734*(1-Elteq!$F$10)","v":204.48987014336558},"8591735039707"]
["TECHNIK SPECIAL - AKCIA","MW 50-C",null,"Matrice k HT131 pro Cu oka stáčená z plechu dle DIN 46234, průřez 50mm2","1ks",204.48987014336558,{"$f":"F735*(1-Elteq!$F$10)","v":204.48987014336558},"8591735039714"]
["TECHNIK SPECIAL - AKCIA","MW 70-C",null,"Matrice k HT131 pro Cu oka stáčená z plechu dle DIN 46234, průřez 70mm2","1ks",204.48987014336558,{"$f":"F736*(1-Elteq!$F$10)","v":204.48987014336558},"8591735039721"]
["TECHNIK SPECIAL - AKCIA","MW 95-C",null,"Matrice k HT131 pro Cu oka stáčená z plechu dle DIN 46234, průřez 95mm2","1ks",204.48987014336558,{"$f":"F737*(1-Elteq!$F$10)","v":204.48987014336558},"8591735048921"]
["TECHNIK SPECIAL - AKCIA","MW120-C",null,"Matrice k HT131 pro Cu oka stáčená z plechu dle DIN 46234, průřez 120mm2","1ks",204.48987014336558,{"$f":"F738*(1-Elteq!$F$10)","v":204.48987014336558},"8591735048938"]
["TECHNIK SPECIAL - AKCIA","MW150-C",null,"Matrice k HT131 pro Cu oka stáčená z plechu dle DIN 46234, průřez 150mm2","1ks",204.48987014336558,{"$f":"F739*(1-Elteq!$F$10)","v":204.48987014336558},"8591735048945"]
["TECHNIK SPECIAL - AKCIA","MW185-C",null,"Matrice k HT131 pro Cu oka stáčená z plechu dle DIN 46234, průřez 185mm2","1ks",204.48987014336558,{"$f":"F740*(1-Elteq!$F$10)","v":204.48987014336558},"8591735048952"]
["TECHNIK SPECIAL - AKCIA","MW240-C",null,"Matrice k HT131 pro Cu oka stáčená z plechu dle DIN 46234, průřez 240mm2","1ks",204.48987014336558,{"$f":"F741*(1-Elteq!$F$10)","v":204.48987014336558},"8591735048969"]
["TECHNIK SPECIAL - AKCIA","PA 10-C",null,"Razník k HT131 pro Cu oka lehčená 10-50mm2","1ks",64.204623475140195,{"$f":"F742*(1-Elteq!$F$10)","v":64.204623475140195},"8591735039349"]
["TECHNIK SPECIAL - AKCIA","PA 24-C",null,"Razník k HT131 pro Cu oka lehčená 70-120mm2","1ks",64.204623475140195,{"$f":"F743*(1-Elteq!$F$10)","v":64.204623475140195},"8591735039486"]
["TECHNIK SPECIAL - AKCIA","PA 48-C",null,"Razník k HT131 pro Cu oka lehčená 150-240mm2","1ks",64.204623475140195,{"$f":"F744*(1-Elteq!$F$10)","v":64.204623475140195},"8591735039462"]
["TECHNIK SPECIAL - AKCIA","PA 60-C",null,"Razník k HT131 pro Cu oka lehčená 300mm2","1ks",70.142623334112699,{"$f":"F745*(1-Elteq!$F$10)","v":70.142623334112699},"8591735039448"]
["TECHNIK SPECIAL - AKCIA","PT 70-C",null,"Čelisti na dutinky 70mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",160.1404336966647,{"$f":"F746*(1-Elteq!$F$10)","v":160.1404336966647},"8591735054540"]
["TECHNIK SPECIAL - AKCIA","PT 95-C",null,"Čelisti na dutinky 95mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",160.1404336966647,{"$f":"F747*(1-Elteq!$F$10)","v":160.1404336966647},"8591735054533"]
["TECHNIK SPECIAL - AKCIA","PT120-C",null,"Čelisti na dutinky 120mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",160.1404336966647,{"$f":"F748*(1-Elteq!$F$10)","v":160.1404336966647},"8591735036980"]
["TECHNIK SPECIAL - AKCIA","PT150-C",null,"Čelisti na dutinky 150mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",160.1404336966647,{"$f":"F749*(1-Elteq!$F$10)","v":160.1404336966647},"8591735036997"]
["TECHNIK SPECIAL - AKCIA","PT185-C",null,"Čelisti na dutinky 185mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",160.1404336966647,{"$f":"F750*(1-Elteq!$F$10)","v":160.1404336966647},"8591735054472"]
["TECHNIK SPECIAL - AKCIA","PT240-C",null,"Čelisti na dutinky 240mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",160.1404336966647,{"$f":"F751*(1-Elteq!$F$10)","v":160.1404336966647},"8591735054526"]
["TECHNIK SPECIAL - AKCIA","PW 10-16 C",null,"Razník k HT131 pro Cu oka stáčená z plechu dle DIN 46234, průřez 10-16mm2","1ks",212.283494958267,{"$f":"F752*(1-Elteq!$F$10)","v":212.283494958267},"8591735048976"]
["TECHNIK SPECIAL - AKCIA","PW 25-35 C",null,"Razník k HT131 pro Cu oka stáčená z plechu dle DIN 46234, průřez 25-35mm2","1ks",212.283494958267,{"$f":"F753*(1-Elteq!$F$10)","v":212.283494958267},"8591735039738"]
["TECHNIK SPECIAL - AKCIA","PW 50-70 C",null,"Razník k HT131 pro Cu oka stáčená z plechu dle DIN 46234, průřez 50-70mm2","1ks",212.283494958267,{"$f":"F754*(1-Elteq!$F$10)","v":212.283494958267},"8591735039745"]
["TECHNIK SPECIAL - AKCIA","PW 95-150 C",null,"Razník k HT131 pro Cu oka stáčená z plechu dle DIN 46234, průřez 95-150mm2","1ks",212.283494958267,{"$f":"F755*(1-Elteq!$F$10)","v":212.283494958267},"8591735048983"]
["TECHNIK SPECIAL - AKCIA","PW185-240 C",null,"Razník k HT131 pro Cu oka stáčená z plechu dle DIN 46234, průřez 185-240mm2","1ks",212.283494958267,{"$f":"F756*(1-Elteq!$F$10)","v":212.283494958267},"8591735048990"]
["TECHNIK SPECIAL - AKCIA","RU  10-C",null,"Čelisti zkružovací na průřezy 10mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.07087373956675,{"$f":"F757*(1-Elteq!$F$10)","v":53.07087373956675},"8591735039684"]
["TECHNIK SPECIAL - AKCIA","RU  16-C",null,"Čelisti zkružovací na průřezy 16mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.07087373956675,{"$f":"F758*(1-Elteq!$F$10)","v":53.07087373956675},"8591735035198"]
["TECHNIK SPECIAL - AKCIA","RU  35/25-C",null,"Čelisti zkružovací na průřezy 35/25mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.07087373956675,{"$f":"F759*(1-Elteq!$F$10)","v":53.07087373956675},"8591735035174"]
["TECHNIK SPECIAL - AKCIA","RU  50/35-C",null,"Čelisti zkružovací na průřezy 50/35mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.07087373956675,{"$f":"F760*(1-Elteq!$F$10)","v":53.07087373956675},"8591735035150"]
["TECHNIK SPECIAL - AKCIA","RU  70/50-C",null,"Čelisti zkružovací na průřezy 70/50mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.07087373956675,{"$f":"F761*(1-Elteq!$F$10)","v":53.07087373956675},"8591735035136"]
["TECHNIK SPECIAL - AKCIA","RU  95/70-C",null,"Čelisti zkružovací na průřezy 95/70mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.07087373956675,{"$f":"F762*(1-Elteq!$F$10)","v":53.07087373956675},"8591735028367"]
["TECHNIK SPECIAL - AKCIA","RU 120/95-C",null,"Čelisti zkružovací na průřezy 120/95mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.07087373956675,{"$f":"F763*(1-Elteq!$F$10)","v":53.07087373956675},"8591735028374"]
["TECHNIK SPECIAL - AKCIA","RU 150/120-C",null,"Čelisti zkružovací na průřezy 150/120mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.07087373956675,{"$f":"F764*(1-Elteq!$F$10)","v":53.07087373956675},"8591735028381"]
["TECHNIK SPECIAL - AKCIA","RU 185/150-C",null,"Čelisti zkružovací na průřezy 185/150mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.07087373956675,{"$f":"F765*(1-Elteq!$F$10)","v":53.07087373956675},"8591735028398"]
["TECHNIK SPECIAL - AKCIA","RU 240/185-C",null,"Čelisti zkružovací na průřezy 240/185mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.07087373956675,{"$f":"F766*(1-Elteq!$F$10)","v":53.07087373956675},"8591735028404"]
["TECHNIK SPECIAL - AKCIA","RU 300/240-C",null,"Čelisti zkružovací na průřezy 300/240mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.07087373956675,{"$f":"F767*(1-Elteq!$F$10)","v":53.07087373956675},"8591735035068"]
["TECHNIK SPECIAL - AKCIA","RU300-C",null,"Čelisti zkružovací na průřezy 300mm2 pro HT131, RH131, RHM132, B131, AP130","1pár",53.07087373956675,{"$f":"F768*(1-Elteq!$F$10)","v":53.07087373956675},"8591735035051"]
["TECHNIK SPECIAL - AKCIA","10 ALU-45",null,"Čelisti na Al 10mm² pro HT45, B45","1pár",32.658999224348769,{"$f":"F769*(1-Elteq!$F$10)","v":32.658999224348769},"8591735026127"]
["TECHNIK SPECIAL - AKCIA","10 CU-45",null,"Čelisti na Cu DIN 25mm², Al 10mm² pro HT45, B45","1pár",32.658999224348769,{"$f":"F770*(1-Elteq!$F$10)","v":32.658999224348769},"8591735026134"]
["TECHNIK SPECIAL - AKCIA","12 ALU-45",null,"Čelisti na Al 16-25mm² pro HT45, B45","1pár",32.658999224348769,{"$f":"F771*(1-Elteq!$F$10)","v":32.658999224348769},"8591735026141"]
["TECHNIK SPECIAL - AKCIA","12 CU-45",null,"Čelisti na Cu DIN 35mm², Al 16-25mm² pro HT45, B45","1pár",32.658999224348769,{"$f":"F772*(1-Elteq!$F$10)","v":32.658999224348769},"8591735026158"]
["TECHNIK SPECIAL - AKCIA","14 ALU-45",null,"Čelisti na Al 35mm² pro HT45, B45","1pár",32.658999224348769,{"$f":"F773*(1-Elteq!$F$10)","v":32.658999224348769},"8591735026165"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK SPECIAL - AKCIA"},"14 CU-45",null,"Čelisti na Cu DIN 50mm², Al 35mm² pro HT45, B45","1pár",32.658999224348769,{"$f":"F774*(1-Elteq!$F$10)","v":32.658999224348769},"8591735026172"]
["TECHNIK SPECIAL - AKCIA","16 ALU-45",null,"Čelisti na Al 50mm2 pro HT45, B45","1pár",32.658999224348769,{"$f":"F775*(1-Elteq!$F$10)","v":32.658999224348769},"8591735026189"]
["TECHNIK SPECIAL - AKCIA","16 CU-45",null,"Čelisti na Cu DIN 70mm2, Al 50mm2 pro HT45, B45","1pár",32.658999224348769,{"$f":"F776*(1-Elteq!$F$10)","v":32.658999224348769},"8591735026196"]
["TECHNIK SPECIAL - AKCIA","18 ALU-45",null,"Čelisti na Al 70mm2 pro HT45, B45","1pár",32.658999224348769,{"$f":"F777*(1-Elteq!$F$10)","v":32.658999224348769},"8591735026202"]
["TECHNIK SPECIAL - AKCIA","18 CU-45",null,"Čelisti na Cu DIN 95mm2, Al 70mm2 pro HT45, B45","1pár",32.658999224348769,{"$f":"F778*(1-Elteq!$F$10)","v":32.658999224348769},"8591735026219"]
["TECHNIK SPECIAL - AKCIA","20 CU-45",null,"Čelisti na Cu DIN 120mm2 pro HT45, B45","1pár",32.658999224348769,{"$f":"F779*(1-Elteq!$F$10)","v":32.658999224348769},"8591735026226"]
["TECHNIK SPECIAL - AKCIA","22 ALU-45",null,"Čelisti na Al 95-120mm2 pro HT45, B45","1pár",32.658999224348769,{"$f":"F780*(1-Elteq!$F$10)","v":32.658999224348769},"8591735026233"]
["TECHNIK SPECIAL - AKCIA","22 CU-45",null,"Čelisti na Cu DIN 150mm2, Al 95-120mm2 pro HT45, B45","1pár",32.658999224348769,{"$f":"F781*(1-Elteq!$F$10)","v":32.658999224348769},"8591735026240"]
["TECHNIK SPECIAL - AKCIA","5 CU-45",null,"Čelisti na Cu DIN 6mm2 pro HT45, B45","1pár",32.658999224348769,{"$f":"F782*(1-Elteq!$F$10)","v":32.658999224348769},"8591735026257"]
["TECHNIK SPECIAL - AKCIA","6 CU-45",null,"Čelisti na Cu DIN 10mm2 pro HT45, B45","1pár",32.658999224348769,{"$f":"F783*(1-Elteq!$F$10)","v":32.658999224348769},"8591735026264"]
["TECHNIK SPECIAL - AKCIA","8 CU-45",null,"Čelisti na Cu DIN 16mm2 pro HT45, B45","1pár",32.658999224348769,{"$f":"F784*(1-Elteq!$F$10)","v":32.658999224348769},"8591735026271"]
["TECHNIK SPECIAL - AKCIA","L  6-45",null,"Čelisti na Cu lehčené 6mm2 pro HT45, B45","1pár",31.545624250791423,{"$f":"F785*(1-Elteq!$F$10)","v":31.545624250791423},"8591735026028"]
["TECHNIK SPECIAL - AKCIA","L 10-45",null,"Čelisti na Cu lehčené 10mm2 pro HT45, B45","1pár",31.545624250791423,{"$f":"F786*(1-Elteq!$F$10)","v":31.545624250791423},"8591735026035"]
["TECHNIK SPECIAL - AKCIA","L 16-45",null,"Čelisti na Cu lehčené 16mm2 pro HT45, B45","1pár",31.545624250791423,{"$f":"F787*(1-Elteq!$F$10)","v":31.545624250791423},"8591735026042"]
["TECHNIK SPECIAL - AKCIA","L 25-45",null,"Čelisti na Cu lehčené 25mm2 pro HT45, B45","1pár",31.545624250791423,{"$f":"F788*(1-Elteq!$F$10)","v":31.545624250791423},"8591735026059"]
["TECHNIK SPECIAL - AKCIA","L 35-45",null,"Čelisti na Cu lehčené 35mm2 pro HT45, B45","1pár",31.545624250791423,{"$f":"F789*(1-Elteq!$F$10)","v":31.545624250791423},"8591735026066"]
["TECHNIK SPECIAL - AKCIA","L 50-45",null,"Čelisti na Cu lehčené 50mm2 pro HT45, B45","1pár",31.545624250791423,{"$f":"F790*(1-Elteq!$F$10)","v":31.545624250791423},"8591735026073"]
["TECHNIK SPECIAL - AKCIA","L 70-45",null,"Čelisti na Cu lehčené 70mm2 pro HT45, B45","1pár",31.545624250791423,{"$f":"F791*(1-Elteq!$F$10)","v":31.545624250791423},"8591735026080"]
["TECHNIK SPECIAL - AKCIA","L 95-45",null,"Čelisti na Cu lehčené 95mm2 pro HT45, B45","1pár",31.545624250791423,{"$f":"F792*(1-Elteq!$F$10)","v":31.545624250791423},"8591735026097"]
["TECHNIK SPECIAL - AKCIA","L120-45",null,"Čelisti na Cu lehčené 120mm2 pro HT45, B45","1pár",31.545624250791423,{"$f":"F793*(1-Elteq!$F$10)","v":31.545624250791423},"8591735026103"]
["TECHNIK SPECIAL - AKCIA","L150-45",null,"Čelisti na Cu lehčené 150mm2 pro HT45, B45","1pár",31.545624250791423,{"$f":"F794*(1-Elteq!$F$10)","v":31.545624250791423},"8591735026110"]
["TECHNIK SPECIAL - AKCIA","10 ALU-50",null,"Čelisti na Al 10mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",34.143499189091891,{"$f":"F795*(1-Elteq!$F$10)","v":34.143499189091891},"8591735026417"]
["TECHNIK SPECIAL - AKCIA","10 CU-50",null,"Čelisti na Cu DIN 25mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",34.143499189091891,{"$f":"F796*(1-Elteq!$F$10)","v":34.143499189091891},"8591735026424"]
["TECHNIK SPECIAL - AKCIA","12 ALU-50",null,"Čelisti na Al 16-25mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",34.143499189091891,{"$f":"F797*(1-Elteq!$F$10)","v":34.143499189091891},"8591735026431"]
["TECHNIK SPECIAL - AKCIA","12 CU-50",null,"Čelisti na Cu DIN 35mm², Al 16-25mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",34.143499189091891,{"$f":"F798*(1-Elteq!$F$10)","v":34.143499189091891},"8591735026448"]
["TECHNIK SPECIAL - AKCIA","14 ALU-50",null,"Čelisti na Al 35mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",34.143499189091891,{"$f":"F799*(1-Elteq!$F$10)","v":34.143499189091891},"8591735026455"]
["TECHNIK SPECIAL - AKCIA","14 CU-50",null,"Čelisti na Cu DIN 50mm², Al 35mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",34.143499189091891,{"$f":"F800*(1-Elteq!$F$10)","v":34.143499189091891},"8591735026462"]
["TECHNIK SPECIAL - AKCIA","16 ALU-50",null,"Čelisti na Al 50mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",34.143499189091891,{"$f":"F801*(1-Elteq!$F$10)","v":34.143499189091891},"8591735026479"]
["TECHNIK SPECIAL - AKCIA","16 CU-50",null,"Čelisti na Cu DIN 70mm², Al 50mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",34.143499189091891,{"$f":"F802*(1-Elteq!$F$10)","v":34.143499189091891},"8591735026486"]
["TECHNIK SPECIAL - AKCIA","18 ALU-50",null,"Čelisti na Al 70mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",34.143499189091891,{"$f":"F803*(1-Elteq!$F$10)","v":34.143499189091891},"8591735026493"]
["TECHNIK SPECIAL - AKCIA","18 CU-50",null,"Čelisti na Cu DIN 95mm², Al 70mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",34.143499189091891,{"$f":"F804*(1-Elteq!$F$10)","v":34.143499189091891},"8591735026509"]
["TECHNIK SPECIAL - AKCIA","20 CU-50",null,"Čelisti na Cu DIN 120mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",34.143499189091891,{"$f":"F805*(1-Elteq!$F$10)","v":34.143499189091891},"8591735026516"]
["TECHNIK SPECIAL - AKCIA","22 ALU-50",null,"Čelisti na Al 95-120mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",34.143499189091891,{"$f":"F806*(1-Elteq!$F$10)","v":34.143499189091891},"8591735026523"]
["TECHNIK SPECIAL - AKCIA","22 CU-50",null,"Čelisti na Cu DIN 150mm²,Al 95-120mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",34.143499189091891,{"$f":"F807*(1-Elteq!$F$10)","v":34.143499189091891},"8591735026530"]
["TECHNIK SPECIAL - AKCIA","25 ALU-50",null,"Čelisti na Al 150mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",34.143499189091891,{"$f":"F808*(1-Elteq!$F$10)","v":34.143499189091891},"8591735026547"]
["TECHNIK SPECIAL - AKCIA","25 CU-50",null,"Čelisti na Cu DIN 185mm², Al 150mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",34.143499189091891,{"$f":"F809*(1-Elteq!$F$10)","v":34.143499189091891},"8591735026554"]
["TECHNIK SPECIAL - AKCIA","28 ALU-50",null,"Čelisti na Al 185mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",34.143499189091891,{"$f":"F810*(1-Elteq!$F$10)","v":34.143499189091891},"8591735026561"]
["TECHNIK SPECIAL - AKCIA","28 CU-50",null,"Čelisti na Cu DIN 240mm², Al 185mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",34.143499189091891,{"$f":"F811*(1-Elteq!$F$10)","v":34.143499189091891},"8591735026578"]
["TECHNIK SPECIAL - AKCIA","32 ALU-50",null,"Čelisti na Al 240mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",34.143499189091891,{"$f":"F812*(1-Elteq!$F$10)","v":34.143499189091891},"8591735026585"]
["TECHNIK SPECIAL - AKCIA","5 CU-50",null,"Čelisti na Cu DIN 6mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",34.143499189091891,{"$f":"F813*(1-Elteq!$F$10)","v":34.143499189091891},"8591735026592"]
["TECHNIK SPECIAL - AKCIA","6 CU-50",null,"Čelisti na Cu DIN 10mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",34.143499189091891,{"$f":"F814*(1-Elteq!$F$10)","v":34.143499189091891},"8591735026608"]
["TECHNIK SPECIAL - AKCIA","8 CU-50",null,"Čelisti na Cu DIN 16mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",34.143499189091891,{"$f":"F815*(1-Elteq!$F$10)","v":34.143499189091891},"8591735026615"]
["TECHNIK SPECIAL - AKCIA","L  6-50",null,"Čelisti na Cu lehčené 6mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",33.364136707601752,{"$f":"F816*(1-Elteq!$F$10)","v":33.364136707601752},"8591735026288"]
["TECHNIK SPECIAL - AKCIA","L 10-50",null,"Čelisti na Cu lehčené 10mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",33.364136707601752,{"$f":"F817*(1-Elteq!$F$10)","v":33.364136707601752},"8591735026295"]
["TECHNIK SPECIAL - AKCIA","L 16-50",null,"Čelisti na Cu lehčené 16mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",33.364136707601752,{"$f":"F818*(1-Elteq!$F$10)","v":33.364136707601752},"8591735026301"]
["TECHNIK SPECIAL - AKCIA","L 25-50",null,"Čelisti na Cu lehčené 25mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",33.364136707601752,{"$f":"F819*(1-Elteq!$F$10)","v":33.364136707601752},"8591735026318"]
["TECHNIK SPECIAL - AKCIA","L 35-50",null,"Čelisti na Cu lehčené 35mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",33.364136707601752,{"$f":"F820*(1-Elteq!$F$10)","v":33.364136707601752},"8591735026325"]
["TECHNIK SPECIAL - AKCIA","L 50-50",null,"Čelisti na Cu lehčené 50mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",33.364136707601752,{"$f":"F821*(1-Elteq!$F$10)","v":33.364136707601752},"8591735026332"]
["TECHNIK SPECIAL - AKCIA","L 70-50",null,"Čelisti na Cu lehčené 70mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",33.364136707601752,{"$f":"F822*(1-Elteq!$F$10)","v":33.364136707601752},"8591735026349"]
["TECHNIK SPECIAL - AKCIA","L 95-50",null,"Čelisti na Cu lehčené 95mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",33.364136707601752,{"$f":"F823*(1-Elteq!$F$10)","v":33.364136707601752},"8591735026356"]
["TECHNIK SPECIAL - AKCIA","L120-50",null,"Čelisti na Cu lehčené 120mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",33.364136707601752,{"$f":"F824*(1-Elteq!$F$10)","v":33.364136707601752},"8591735026363"]
["TECHNIK SPECIAL - AKCIA","L150-50",null,"Čelisti na Cu lehčené 150mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",33.364136707601752,{"$f":"F825*(1-Elteq!$F$10)","v":33.364136707601752},"8591735026370"]
["TECHNIK SPECIAL - AKCIA","L185-50",null,"Čelisti na Cu lehčené 185mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",33.364136707601752,{"$f":"F826*(1-Elteq!$F$10)","v":33.364136707601752},"8591735026387"]
["TECHNIK SPECIAL - AKCIA","L240-50",null,"Čelisti na Cu lehčené 240mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",33.364136707601752,{"$f":"F827*(1-Elteq!$F$10)","v":33.364136707601752},"8591735026394"]
["TECHNIK SPECIAL - AKCIA","RU  10-50",null,"Čelisti zkružovací na průřezy 10mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",48.20913635503301,{"$f":"F828*(1-Elteq!$F$10)","v":48.20913635503301},"8591735029036"]
["TECHNIK SPECIAL - AKCIA","RU  16-50",null,"Čelisti zkružovací na průřezy 16mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",48.20913635503301,{"$f":"F829*(1-Elteq!$F$10)","v":48.20913635503301},"8591735029043"]
["TECHNIK SPECIAL - AKCIA","RU  35/25-50",null,"Čelisti zkružovací na průřezy 35/25mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",48.20913635503301,{"$f":"F830*(1-Elteq!$F$10)","v":48.20913635503301},"8591735029050"]
["TECHNIK SPECIAL - AKCIA","RU  50/35-50",null,"Čelisti zkružovací na průřezy 50/35mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",48.20913635503301,{"$f":"F831*(1-Elteq!$F$10)","v":48.20913635503301},"8591735029067"]
["TECHNIK SPECIAL - AKCIA","RU  70/50-50",null,"Čelisti zkružovací na průřezy 70/50mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",48.20913635503301,{"$f":"F832*(1-Elteq!$F$10)","v":48.20913635503301},"8591735028350"]
["TECHNIK SPECIAL - AKCIA","RU  95/70-50",null,"Čelisti zkružovací na průřezy 95/70mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",48.20913635503301,{"$f":"F833*(1-Elteq!$F$10)","v":48.20913635503301},"8591735029074"]
["TECHNIK SPECIAL - AKCIA","RU 120/95-50",null,"Čelisti zkružovací na průřezy 120/95mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",48.20913635503301,{"$f":"F834*(1-Elteq!$F$10)","v":48.20913635503301},"8591735028343"]
["TECHNIK SPECIAL - AKCIA","RU 150/120-50",null,"Čelisti zkružovací na průřezy 150/120mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",48.20913635503301,{"$f":"F835*(1-Elteq!$F$10)","v":48.20913635503301},"8591735029081"]
["TECHNIK SPECIAL - AKCIA","RU 185/150-50",null,"Čelisti zkružovací na průřezy 185/150mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",48.20913635503301,{"$f":"F836*(1-Elteq!$F$10)","v":48.20913635503301},"8591735029098"]
["TECHNIK SPECIAL - AKCIA","RU 240/185-50",null,"Čelisti zkružovací na průřezy 240/185mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",48.20913635503301,{"$f":"F837*(1-Elteq!$F$10)","v":48.20913635503301},"8591735028336"]
[{"$f":"REPLACE(CELL(\"Filename\",$A$1),1,FIND(\"]\",CELL(\"filename\",$A$1)),\"\")","v":"TECHNIK SPECIAL - AKCIA"},"RU 300/240-50",null,"Čelisti zkružovací na průřezy 300/240mm² pro K18, HT51, HT60, RH50, B50, B62","1pár",48.20913635503301,{"$f":"F838*(1-Elteq!$F$10)","v":48.20913635503301},"8591735031442"]
["TECHNIK SPECIAL - AKCIA","L130-D 10",null,"Čelisti na Cu DIN 10mm2 pro lisovací hlavici LH130","1pár",35.62799915383502,{"$f":"F839*(1-Elteq!$F$10)","v":35.62799915383502},"8591735054380"]
["TECHNIK SPECIAL - AKCIA","L130-L 10",null,"Čelisti na Cu lehčené 10mm2 pro lisovací hlavici LH130","1pár",38.040311596542601,{"$f":"F840*(1-Elteq!$F$10)","v":38.040311596542601},"8591735054373"]
["TECHNIK SPECIAL - AKCIA","A3-MO 01475/28",null,"Aretace k PP pro neizolované konektory 2,8x0,8mm","1ks",54.926498695495653,{"$f":"F841*(1-Elteq!$F$10)","v":54.926498695495653},"8591735039271"]
["TECHNIK SPECIAL - AKCIA","A3-MO 056/68",null,"Aretace k PP pro neizolované konektory 6,3x0,8mm","1ks",54.926498695495653,{"$f":"F842*(1-Elteq!$F$10)","v":54.926498695495653},"8591735035983"]
["TECHNIK SPECIAL - AKCIA","A3-OI 056/68",null,"Aretace k PP pro izolované konektory 6,3x0,8mm","1ks",54.926498695495653,{"$f":"F843*(1-Elteq!$F$10)","v":54.926498695495653},"8591735037444"]
["TECHNIK SPECIAL - AKCIA","C3-BP 0515",null,"Čelisti k PP12470 a LK3 na mosazné objímky, průřez 0,5-1,5mm2 s bočním připojením","1pár",405.26849037487335,{"$f":"F844*(1-Elteq!$F$10)","v":405.26849037487335},"8591735036096"]
["TECHNIK SPECIAL - AKCIA","C3-BP 1525",null,"Čelisti k PP12470 a LK3 na mosazné objímky, průřez 1,5-2,5mm2 s bočním připojením","1pár",405.26849037487335,{"$f":"F845*(1-Elteq!$F$10)","v":405.26849037487335},"8591735036102"]
["TECHNIK SPECIAL - AKCIA","C3-BPI 1525",null,"Čelisti k PP12470 a LK3 na objímky izolované, průřez 1,5-2,5mm2 s bočním připojením","1pár",374.83624109763929,{"$f":"F846*(1-Elteq!$F$10)","v":374.83624109763929},"8591735036119"]
["TECHNIK SPECIAL - AKCIA","C3-D 01425",null,"Čelisti k PP12470 a LK3 na dutinky, průřez 0,14-2,5mm2","1pár",201.52087021387933,{"$f":"F847*(1-Elteq!$F$10)","v":201.52087021387933},"8591735036126"]
["TECHNIK SPECIAL - AKCIA","C3-D 0256",null,"Čelisti k PP12470 a LK3 na dutinky, průřez 0,25-6mm2","1pár",230.83974451755606,{"$f":"F848*(1-Elteq!$F$10)","v":230.83974451755606},"8591735036133"]
["TECHNIK SPECIAL - AKCIA","C3-D 2535",null,"Čelisti k PP12470 a LK3 na dutinky, průřez 25 a 35mm2","1pár",239.74674430601482,{"$f":"F849*(1-Elteq!$F$10)","v":239.74674430601482},"8591735036157"]
["TECHNIK SPECIAL - AKCIA","C3-D 2550",null,"Čelisti k PP12470 a LK3 na dutinky, průřez 25 a 50mm2","1pár",239.74674430601482,{"$f":"F850*(1-Elteq!$F$10)","v":239.74674430601482},"8591735036164"]
["TECHNIK SPECIAL - AKCIA","C3-D 616",null,"Čelisti k PP12470 a LK3 na dutinky, průřez 6-16mm2","1pár",230.83974451755606,{"$f":"F851*(1-Elteq!$F$10)","v":230.83974451755606},"8591735036140"]
["TECHNIK SPECIAL - AKCIA","C3-MO 01415",null,"Čelisti k PP12470 a LK3 na mosazné objímky, průřez 0,14-1,5mm2 / 2,8 a 4,8mm","1pár",422.15467747382638,{"$f":"F852*(1-Elteq!$F$10)","v":422.15467747382638},"8591735036171"]
["TECHNIK SPECIAL - AKCIA","C3-MO 056",null,"Čelisti k PP12470 a LK3 na mosazné objímky, průřez 0,5-6mm2 / 4,8 a 6,3mm","1pár",374.83624109763929,{"$f":"F853*(1-Elteq!$F$10)","v":374.83624109763929},"8591735035976"]
["TECHNIK SPECIAL - AKCIA","C3-OI 02525",null,"Čelisti k PP12470 a LK3 na koncovky izolované, průřez 0,25-2,5mm2","1pár",239.74674430601482,{"$f":"F854*(1-Elteq!$F$10)","v":239.74674430601482},"8591735036188"]
["TECHNIK SPECIAL - AKCIA","C3-OI 056",null,"Čelisti k PP12470 a LK3 na koncovky izolované, průřez 0,5-6mm2","1pár",174.05762086613151,{"$f":"F855*(1-Elteq!$F$10)","v":174.05762086613151},"8591735035877"]
["TECHNIK SPECIAL - AKCIA","C3-OL 156",null,"Čelisti k PP12470 a LK3 na oka lehčená, průřez 1-6mm2","1pár",194.65505787694238,{"$f":"F856*(1-Elteq!$F$10)","v":194.65505787694238},"8591735036195"]
["TECHNIK SPECIAL - AKCIA","C3-ON 056",null,"Čelisti k PP12470 a LK3 na oka neizolovaná, průřez 0,5-6mm2","1pár",194.65505787694238,{"$f":"F857*(1-Elteq!$F$10)","v":194.65505787694238},"8591735035884"]
["TECHNIK SPECIAL - AKCIA","C3-ON10",null,"Čelisti k PP12470 a LK3 na oka neizolovaná, průřez 10mm2","1pár",194.65505787694238,{"$f":"F858*(1-Elteq!$F$10)","v":194.65505787694238},"8591735036201"]
["TECHNIK SPECIAL - AKCIA","C3-ON16",null,"Čelisti k PP12470 a LK3 na oka neizolovaná, průřez 16mm2","1pár",194.65505787694238,{"$f":"F859*(1-Elteq!$F$10)","v":194.65505787694238},"8591735036218"]
["TECHNIK SPECIAL - AKCIA","C3-PT",null,"Čelisti k PP12470 a LK3, pouze polotovar pro vlastní výrobu čelisti","1pár",166.44955854682297,{"$f":"F860*(1-Elteq!$F$10)","v":166.44955854682297},"8591735035891"]
["TECHNIK SPECIAL - AKCIA","C3-SK 0525",null,"Čelisti k PP12470 a LK3 na kontakty Walther, průřez 0,5-2,5mm2","1pár",333.82692957161044,{"$f":"F861*(1-Elteq!$F$10)","v":333.82692957161044},"8591735035907"]
["TECHNIK SPECIAL - AKCIA","C3-SK 0754",null,"Čelisti k PP12470 a LK3 na soustružené kontakty, průřez 0,75-4mm2","1pár",374.83624109763929,{"$f":"F862*(1-Elteq!$F$10)","v":374.83624109763929},"8591735035914"]
["TECHNIK SPECIAL - AKCIA","C3-X1",null,"Čelisti k PP12470 a LK3 na koaxiální BNC konektory RG 58, 59, 62, 71","1pár",198.73743277998597,{"$f":"F863*(1-Elteq!$F$10)","v":198.73743277998597},"8591735036225"]
["TECHNIK SPECIAL - AKCIA","C3-X2",null,"Čelisti k PP12470 a LK3 na koaxiální BNC konektory RG 58, 174","1pár",239.74674430601482,{"$f":"F864*(1-Elteq!$F$10)","v":239.74674430601482},"8591735036232"]
["TECHNIK SPECIAL - AKCIA","C6-ON 410",null,"Čelisti lisovací CSV10-66 k pneumatickému lisu PP600 na oka a spojky bez izolace, průřez 4-10mm2","1pár",166.07843355563719,{"$f":"F865*(1-Elteq!$F$10)","v":166.07843355563719},"8591735054687"]
["TECHNIK SPECIAL - AKCIA","C6-OI 0525",null,"Čelisti lisovací CSVC10 k pneumatickému lisu PP600 na koncovky s izolací, průřez 0,5-2,5mm2","1pár",158.84149622751445,{"$f":"F866*(1-Elteq!$F$10)","v":158.84149622751445},"8591735054885"]
["TECHNIK SPECIAL - AKCIA","38 CU-1000",null,"Čelisti na Cu DIN 400mm2 pro hydraulickou lisovací hlavici RHU 1000","1pár",718.86910792685865,{"$f":"F867*(1-Elteq!$F$10)","v":718.86910792685865},""]
["TECHNIK SPECIAL - AKCIA","44 CU-1000",null,"Čelisti na Cu DIN 625mm2 pro hydraulickou lisovací hlavici RHU 1000","1pár",718.86910792685865,{"$f":"F868*(1-Elteq!$F$10)","v":718.86910792685865},""]
["TECHNIK SPECIAL - AKCIA","60 CU-1000",null,"Čelisti na Cu DIN 1200mm2 pro hydraulickou lisovací hlavici RHU 1000","1pár",718.86910792685865,{"$f":"F869*(1-Elteq!$F$10)","v":718.86910792685865},""]
["TECHNIK SPECIAL - AKCIA","18 ALU-450",null,"Čelisti lisovací na Al 70mm2 pro hydraulickou hlavici RHU 450","1pár",137.13068424314625,{"$f":"F870*(1-Elteq!$F$10)","v":137.13068424314625},"8591735039110"]
["TECHNIK SPECIAL - AKCIA","22 ALU-450",null,"Čelisti lisovací na Al 95-120mm2 pro hydraulickou hlavici RHU 450","1pár",137.13068424314625,{"$f":"F871*(1-Elteq!$F$10)","v":137.13068424314625},"8591735039660"]
["TECHNIK SPECIAL - AKCIA","28 CU-450",null,"Čelisti lisovací na Cu DIN 240mm2, Al 185mm2 pro hydraulickou hlavici RHU 450","1pár",137.13068424314625,{"$f":"F872*(1-Elteq!$F$10)","v":137.13068424314625},"8591735039141"]
["TECHNIK SPECIAL - AKCIA","32 ALU-450",null,"Čelisti lisovací na Al 240mm2 pro hydraulickou hlavici RHU 450","1pár",137.13068424314625,{"$f":"F873*(1-Elteq!$F$10)","v":137.13068424314625},"8591735039097"]
["TECHNIK SPECIAL - AKCIA","32 CU-450",null,"Čelisti lisovací na Cu DIN 300mm2, Al 240mm2 pro hydraulickou hlavici RHU 450","1pár",137.13068424314625,{"$f":"F874*(1-Elteq!$F$10)","v":137.13068424314625},"8591735039134"]
["TECHNIK SPECIAL - AKCIA","34 ALU-450",null,"Čelisti lisovací na Al 300mm2 pro hydraulickou hlavici RHU 450","1pár",137.13068424314625,{"$f":"F875*(1-Elteq!$F$10)","v":137.13068424314625},"8591735039165"]
["TECHNIK SPECIAL - AKCIA","38 CU-450",null,"Čelisti lisovací na Cu DIN 400mm2 pro hydraulickou hlavici RHU 450","1pár",137.13068424314625,{"$f":"F876*(1-Elteq!$F$10)","v":137.13068424314625},"8591735039073"]
["TECHNIK SPECIAL - AKCIA","42 ALU-450",null,"Čelisti lisovací na Al 400mm2 pro hydraulickou hlavici RHU 450","1pár",137.13068424314625,{"$f":"F877*(1-Elteq!$F$10)","v":137.13068424314625},"8591735039103"]
["TECHNIK SPECIAL - AKCIA","42 CU-450",null,"Čelisti lisovací na Cu DIN 500mm2, Al 400mm2 pro hydraulickou hlavici RHU 450","1pár",137.13068424314625,{"$f":"F878*(1-Elteq!$F$10)","v":137.13068424314625},"8591735037970"]
["TECHNIK SPECIAL - AKCIA","44 ALU-450",null,"Čelisti lisovací na Al 500mm2 pro hydraulickou hlavici RHU 450","1pár",137.13068424314625,{"$f":"F879*(1-Elteq!$F$10)","v":137.13068424314625},"8591735037246"]
["TECHNIK SPECIAL - AKCIA","44 CU-450",null,"Čelisti lisovací na Cu DIN 625mm2, Al 500mm2 pro hydraulickou hlavici RHU 450","1pár",137.13068424314625,{"$f":"F880*(1-Elteq!$F$10)","v":137.13068424314625},"8591735037222"]
["TECHNIK SPECIAL - AKCIA","52 ALU-450",null,"Čelisti lisovací na Al 625mm2 pro hydraulickou hlavici RHU 450","1pár",137.13068424314625,{"$f":"F881*(1-Elteq!$F$10)","v":137.13068424314625},"8591735037352"]
["TECHNIK SPECIAL - AKCIA","52 CU-450",null,"Čelisti lisovací na Cu DIN 800mm2, Al 625mm2 pro hydraulickou hlavici RHU 450","1pár",137.13068424314625,{"$f":"F882*(1-Elteq!$F$10)","v":137.13068424314625},"8591735037420"]
["TECHNIK SPECIAL - AKCIA","58 ALU-450",null,"Čelisti lisovací na Al 800mm2 pro hydraulickou hlavici RHU 450","1pár",137.13068424314625,{"$f":"F883*(1-Elteq!$F$10)","v":137.13068424314625},"8591735037963"]
["TECHNIK SPECIAL - AKCIA","58 CU-450",null,"Čelisti lisovací na Cu DIN 1000mm2, Al 800mm2 pro hydraulickou hlavici RHU 450","1pár",137.13068424314625,{"$f":"F884*(1-Elteq!$F$10)","v":137.13068424314625},"8591735039127"]
["TECHNIK SPECIAL - AKCIA","60 ALU-450",null,"Čelisti lisovací na Al 1000mm2 pro hydraulickou hlavici RHU 450","1pár",137.13068424314625,{"$f":"F885*(1-Elteq!$F$10)","v":137.13068424314625},"8591735037956"]
["TECHNIK SPECIAL - AKCIA","AU 450-130 D",null,"Adaptér k RHU 450 pro čelisti typ \"C\"","1pár",248.0970566076949,{"$f":"F886*(1-Elteq!$F$10)","v":248.0970566076949},"8591735042554"]
["TECHNIK SPECIAL - AKCIA","34 CU-520",null,"Čelisti lisovací na Al 300mm2 pro hydraulickou hlavici RHU 520","1pár",325.10549227874458,{"$f":"F887*(1-Elteq!$F$10)","v":325.10549227874458},"8591735039509"]
["TECHNIK SPECIAL - AKCIA","38 CU-520",null,"Čelisti lisovací na Cu DIN 400mm2 pro hydraulickou hlavici RHU 520","1pár",325.10549227874458,{"$f":"F888*(1-Elteq!$F$10)","v":325.10549227874458},"8591735039295"]
["TECHNIK SPECIAL - AKCIA","42 CU-520",null,"Čelisti lisovací na Cu DIN 500mm2, Al 400mm2 pro hydraulickou hlavici RHU 520","1pár",325.10549227874458,{"$f":"F889*(1-Elteq!$F$10)","v":325.10549227874458},"8591735039226"]
["TECHNIK SPECIAL - AKCIA","44 CU-520",null,"Čelisti lisovací na Cu DIN 625mm2, Al 500mm2 pro hydraulickou hlavici RHU 520","1pár",325.10549227874458,{"$f":"F890*(1-Elteq!$F$10)","v":325.10549227874458},"8591735039288"]
["TECHNIK SPECIAL - AKCIA","48 CU-520",null,"Čelisti lisovací speciální na Cu DIN / Al pro hydraulickou hlavici RHU 520","1pár",325.10549227874458,{"$f":"F891*(1-Elteq!$F$10)","v":325.10549227874458},"8591735039301"]
["TECHNIK SPECIAL - AKCIA","52 CU-520",null,"Čelisti lisovací na Cu DIN 800mm2, Al 625mm2 pro hydraulickou hlavici RHU 520","1pár",325.10549227874458,{"$f":"F892*(1-Elteq!$F$10)","v":325.10549227874458},"8591735039219"]
["TECHNIK SPECIAL - AKCIA","58 CU-520",null,"Čelisti lisovací na Cu DIN 1000mm2, Al 800mm2 pro hydraulickou hlavici RHU 520","1pár",325.10549227874458,{"$f":"F893*(1-Elteq!$F$10)","v":325.10549227874458},"8591735039264"]
["TECHNIK SPECIAL - AKCIA","60 CU-520",null,"Čelisti lisovací na Al 1000mm2 pro hydraulickou hlavici RHU 520","1pár",325.10549227874458,{"$f":"F894*(1-Elteq!$F$10)","v":325.10549227874458},"8591735039400"]
["TECHNIK SPECIAL - AKCIA","AU 520-130 C",null,"Adaptér k RHU 520 pro čelisti typ \"C\"","1pár",506.95673795977746,{"$f":"F895*(1-Elteq!$F$10)","v":506.95673795977746},"8591735048556"]
["TECHNIK SPECIAL - AKCIA","28 ALU-19",null,"Čelisti na Al 185mm2 pro K19, MHP10/300","1pár",50.658561296859169,{"$f":"F896*(1-Elteq!$F$10)","v":50.658561296859169},"8591735047610"]
["TECHNIK SPECIAL - AKCIA","28 CU-19",null,"Čelisti na Cu DIN 240mm2, Al 185mm2 pro K19, MHP10/300","1pár",50.658561296859169,{"$f":"F897*(1-Elteq!$F$10)","v":50.658561296859169},"8591735047627"]
["TECHNIK SPECIAL - AKCIA","L300-19",null,"Čelisti na Cu lehčené 300mm2 pro K19, MHP10/300","1pár",69.029248360555357,{"$f":"F898*(1-Elteq!$F$10)","v":69.029248360555357},"8591735047603"]
[null,null,null,null,null,null,{"$f":"F899*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F900*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F901*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F902*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F903*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F904*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F905*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F906*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F907*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F908*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F909*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F910*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F911*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F912*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F913*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F914*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F915*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F916*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F917*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F918*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F919*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F920*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F921*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F922*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F923*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F924*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F925*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F926*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F927*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F928*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F929*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F930*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F931*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F932*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F933*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F934*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F935*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F936*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F937*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F938*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F939*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F940*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F941*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F942*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F943*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F944*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F945*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F946*(1-Elteq!$F$10)","v":0}]
[null,null,null,null,null,null,{"$f":"F947*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F965*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F1029*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F1093*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F1157*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F1221*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F1285*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F1349*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F1413*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F1477*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F1541*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F1605*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F1669*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F1733*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F1797*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F1861*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F1925*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F1989*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F2053*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F2117*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F2181*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F2245*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F2309*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F2373*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F2437*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F2501*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F2565*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F2629*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F2693*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F2757*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F2821*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F2885*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F2949*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F3013*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F3077*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F3141*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F3205*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F3269*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F3333*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F3397*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F3461*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F3525*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F3589*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F3653*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F3717*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F3781*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F3845*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F3909*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F3973*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F4037*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F4101*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F4165*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F4229*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F4293*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F4357*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F4421*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F4485*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F4549*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F4613*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F4677*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F4741*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F4805*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F4869*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F4933*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F4997*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F5061*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F5125*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F5189*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F5253*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F5317*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F5381*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F5445*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F5509*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F5573*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F5637*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F5701*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F5765*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F5829*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F5893*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F5957*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F6021*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F6085*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F6149*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F6213*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F6277*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,{"$f":"F6341*(1-$G$2)","v":0}]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]
[null,null,null,null,null,null,0]

{"sheet":"List","index":9,"n_rows":14298,"n_cols":2,"rows_kept":14298,"cut":false,"hidden":true,"merged":[]}
["Sheet name","Prod"]
["ANAMET-M",432310]
["ANAMET-M",555810]
["ANAMET-M",559730]
["ANAMET-M",559830]
["ANAMET-M",572610]
["ANAMET-M",594010]
["ANAMET-S",1070102]
["ANAMET-S",1070122]
["ANAMET-S",1070162]
["ANAMET-S",1070202]
["ANAMET-S",1070262]
["ANAMET-S",1070352]
["ANAMET-S",1077102]
["ANAMET-S",1077122]
["ANAMET-S",1077162]
["ANAMET-S",1077202]
["ANAMET-S",1077262]
["ANAMET-S",1077352]
["ANAMET-S",1077402]
["ANAMET-S",1077502]
["ANAMET-M",2227031]
["ANAMET-M",2560120]
["ANAMET-M",2560150]
["ANAMET-M",2560160]
["ANAMET-M",2560170]
["ANAMET-M",2560200]
["ANAMET-M",2560250]
["ANAMET-M",2560320]
["ANAMET-S",2560400]
["ANAMET-S",2560500]
["ANAMET-S",2560600]
["ANAMET-M",2561120]
["ANAMET-M",2561150]
["ANAMET-M",2561160]
["ANAMET-M",2561170]
["ANAMET-M",2561200]
["ANAMET-M",2561250]
["ANAMET-M",2561320]
["ANAMET-S",2561400]
["ANAMET-S",2561500]
["ANAMET-S",2561600]
["ANAMET-M",2601100]
["ANAMET-M",2601110]
["ANAMET-M",2601120]
["ANAMET-M",2601150]
["ANAMET-M",2601160]
["ANAMET-M",2601170]
["ANAMET-M",2601180]
["ANAMET-M",2601200]
["ANAMET-M",2601250]
["ANAMET-M",2601320]
["ANAMET-S",2601400]
["ANAMET-S",2601500]
["ANAMET-S",2601600]
["ANAMET-M",2602070]
["ANAMET-M",2602090]
["ANAMET-M",2602110]
["ANAMET-M",2602130]
["ANAMET-M",2602160]
["ANAMET-M",2602210]
["ANAMET-M",2602290]
["ANAMET-S",2602360]
["ANAMET-S",2602480]
["ANAMET-M",2603110]
["ANAMET-M",2603120]
["ANAMET-M",2603160]
["ANAMET-M",2603170]
["ANAMET-M",2603200]
["ANAMET-M",2603250]
["ANAMET-M",2603320]
["ANAMET-S",2603400]
["ANAMET-S",2603500]
["ANAMET-M",2605070]
["ANAMET-M",2605090]
["ANAMET-M",2605120]
["ANAMET-M",2605130]
["ANAMET-M",2611100]
["ANAMET-M",2611110]
["ANAMET-M",2611120]
["ANAMET-M",2611150]
["ANAMET-M",2611160]
["ANAMET-M",2611170]
["ANAMET-M",2611180]
["ANAMET-M",2611200]
["ANAMET-M",2611250]
["ANAMET-M",2611320]
["ANAMET-S",2611400]
["ANAMET-S",2611500]
["ANAMET-S",2611600]
["ANAMET-M",2612070]
["ANAMET-M",2612090]
["ANAMET-M",2612110]
["ANAMET-M",2612130]
["ANAMET-M",2612160]
["ANAMET-M",2612210]
["ANAMET-M",2612290]
["ANAMET-S",2612360]
["ANAMET-S",2612480]
["ANAMET-M",2615070]
["ANAMET-M",2615090]
["ANAMET-M",2615120]
["ANAMET-M",2615130]
["ANAMET-M",2622100]
["ANAMET-M",2622120]
["ANAMET-M",2622160]
["ANAMET-M",2622180]
["ANAMET-M",2622200]
["ANAMET-M",2622250]
["ANAMET-M",2622320]
["ANAMET-S",2622400]
["ANAMET-S",2622500]
["ANAMET-M",2630160]
["ANAMET-M",2630200]
["ANAMET-M",2630250]
["ANAMET-M",2630320]
["ANAMET-M",2631160]
["ANAMET-M",2631200]
["ANAMET-M",2631250]
["ANAMET-M",2631320]
["ANAMET-M",2633120]
["ANAMET-M",2633160]
["ANAMET-M",2633200]
["ANAMET-M",2633260]
["ANAMET-M",2633350]
["ANAMET-M",2633400]
["ANAMET-M",2633500]
["ANAMET-M",2634120]
["ANAMET-M",2634160]
["ANAMET-M",2634200]
["ANAMET-M",2634260]
["ANAMET-M",2634350]
["ANAMET-M",2634400]
["ANAMET-M",2634500]
["ANAMET-M",2641100]
["ANAMET-M",2641120]
["ANAMET-M",2641160]
["ANAMET-M",2641180]
["ANAMET-M",2641200]
["ANAMET-M",2641250]
["ANAMET-M",2641320]
["ANAMET-S",2641400]
["ANAMET-S",2641500]
["ANAMET-M",2651160]
["ANAMET-M",2651161]
["ANAMET-M",2651200]
["ANAMET-M",2651201]
["ANAMET-M",2651250]
["ANAMET-M",2651251]
["ANAMET-M",2651320]
["ANAMET-M",2651400]
["ANAMET-M",2651500]
["ANAMET-M",2651630]
["ANAMET-M",2653160]
["ANAMET-M",2653161]
["ANAMET-M",2653200]
["ANAMET-M",2653201]
["ANAMET-M",2653250]
["ANAMET-M",2653251]
["ANAMET-M",2653320]
["ANAMET-M",2653400]
["ANAMET-M",2653501]
["ANAMET-M",2653630]
["ANAMET-M",2655090]
["ANAMET-M",2655110]
["ANAMET-M",2655131]
["ANAMET-M",2655160]
["ANAMET-M",2655210]
["ANAMET-M",2655290]
["ANAMET-M",2655360]
["ANAMET-M",2655480]
["ANAMET-M",2657090]
["ANAMET-M",2657110]
["ANAMET-M",2657130]
["ANAMET-M",2657160]
["ANAMET-M",2657210]
["ANAMET-M",2657290]
["ANAMET-M",2657360]
["ANAMET-M",2657480]
["ANAMET-M",2661090]
["ANAMET-M",2661110]
["ANAMET-M",2661150]
["ANAMET-M",2661160]
["ANAMET-M",2661210]
["ANAMET-M",2661290]
["ANAMET-M",2661360]
["ANAMET-M",2661420]
["ANAMET-M",2661480]
["ANAMET-M",2662070]
["ANAMET-M",2662090]
["ANAMET-M",2662110]
["ANAMET-M",2662160]
["ANAMET-M",2662210]
["ANAMET-M",2662290]
["ANAMET-M",2662360]
["ANAMET-M",2662420]
["ANAMET-M",2664160]
["ANAMET-M",2664200]
["ANAMET-M",2664250]
["ANAMET-M",2664320]
["ANAMET-M",2664400]
["ANAMET-M",2664500]
["ANAMET-M",2664630]
["ANAMET-M",2665120]
["ANAMET-M",2665160]
["ANAMET-M",2665200]
["ANAMET-M",2665250]
["ANAMET-M",2665320]
["ANAMET-M",2665400]
["ANAMET-M",2665500]
["ANAMET-M",2666120]
["ANAMET-M",2666160]
["ANAMET-M",2666200]
["ANAMET-M",2666250]
["ANAMET-M",2666320]
["ANAMET-M",2666400]
["ANAMET-M",2666500]
["ANAMET-M",2666630]
["ANAMET-M",2667070]
["ANAMET-M",2667090]
["ANAMET-M",2667110]
["ANAMET-M",2667130]
["ANAMET-M",2667160]
["ANAMET-M",2667210]
["ANAMET-M",2667290]
["ANAMET-M",2667360]
["ANAMET-M",2667480]
["ANAMET-M",2668120]
["ANAMET-M",2668170]
["ANAMET-M",2668230]
["ANAMET-M",2668290]
["ANAMET-M",2668360]
["ANAMET-M",2670160]
["ANAMET-M",2670161]
["ANAMET-M",2670200]
["ANAMET-M",2670201]
["ANAMET-M",2670202]
["ANAMET-M",2670250]
["ANAMET-M",2670251]
["ANAMET-M",2670320]
["ANAMET-M",2671090]
["ANAMET-M",2671110]
["ANAMET-M",2671130]
["ANAMET-M",2671131]
["ANAMET-M",2671160]
["ANAMET-M",2671210]
["ANAMET-M",2671290]
["ANAMET-M",2672070]
["ANAMET-M",2672100]
["ANAMET-M",2672120]
["ANAMET-M",2672170]
["ANAMET-M",2672230]
["ANAMET-M",2672290]
["ANAMET-M",2672360]
["ANAMET-M",2672480]
["ANAMET-M",2673070]
["ANAMET-M",2673100]
["ANAMET-M",2673120]
["ANAMET-M",2673170]
["ANAMET-M",2673230]
["ANAMET-M",2673290]
["ANAMET-M",2673360]
["ANAMET-M",2673480]
["ANAMET-M",2674070]
["ANAMET-M",2674100]
["ANAMET-M",2674120]
["ANAMET-M",2674170]
["ANAMET-M",2674230]
["ANAMET-M",2674290]
["ANAMET-M",2674360]
["ANAMET-M",2674480]
["ANAMET-M",2675000]
["ANAMET-M",2675010]
["ANAMET-M",2675070]
["ANAMET-M",2675100]
["ANAMET-M",2675120]
["ANAMET-M",2675170]
["ANAMET-M",2675230]
["ANAMET-M",2675290]
["ANAMET-M",2675360]
["ANAMET-M",2675480]
["ANAMET-M",2676100]
["ANAMET-M",2676130]
["ANAMET-M",2676170]
["ANAMET-M",2676220]
["ANAMET-M",2677100]
["ANAMET-M",2677110]
["ANAMET-M",2677130]
["ANAMET-M",2677140]
["ANAMET-M",2677170]
["ANAMET-M",2678170]
["ANAMET-M",2678200]
["ANAMET-M",2678210]
["ANAMET-M",2678220]
["ANAMET-M",2680120]
["ANAMET-M",2680121]
["ANAMET-M",2680160]
["ANAMET-M",2680161]
["ANAMET-M",2680200]
["ANAMET-M",2680201]
["ANAMET-M",2680250]
["ANAMET-M",2680251]
["ANAMET-M",2680320]
["ANAMET-M",2680400]
["ANAMET-M",2680500]
["ANAMET-M",2680630]
["ANAMET-M",2681120]
["ANAMET-M",2681121]
["ANAMET-M",2681160]
["ANAMET-M",2681161]
["ANAMET-M",2681200]
["ANAMET-M",2681201]
["ANAMET-M",2681250]
["ANAMET-M",2681251]
["ANAMET-M",2681320]
["ANAMET-M",2681400]
["ANAMET-M",2681500]
["ANAMET-M",2681630]
["ANAMET-M",2682160]
["ANAMET-M",2682161]
["ANAMET-M",2682200]
["ANAMET-M",2682201]
["ANAMET-M",2682250]
["ANAMET-M",2682251]
["ANAMET-M",2682320]
["ANAMET-M",2682321]
["ANAMET-M",2682400]
["ANAMET-M",2682401]
["ANAMET-M",2682500]
["ANAMET-M",2682501]
["ANAMET-M",2682630]
["ANAMET-M",2683160]
["ANAMET-M",2683161]
["ANAMET-M",2683200]
["ANAMET-M",2683201]
["ANAMET-M",2683250]
["ANAMET-M",2683251]
["ANAMET-M",2683320]
["ANAMET-M",2683321]
["ANAMET-M",2683400]
["ANAMET-M",2683401]
["ANAMET-M",2683500]
["ANAMET-M",2683501]
["ANAMET-M",2683630]
["ANAMET-M",2684070]
["ANAMET-M",2684071]
["ANAMET-M",2684090]
["ANAMET-M",2684091]
["ANAMET-M",2684110]
["ANAMET-M",2684111]
["ANAMET-M",2684130]
["ANAMET-M",2684131]
["ANAMET-M",2684160]
["ANAMET-M",2684210]
["ANAMET-M",2684290]
["ANAMET-M",2684360]
["ANAMET-M",2684480]
["ANAMET-M",2685070]
["ANAMET-M",2685071]
["ANAMET-M",2685090]
["ANAMET-M",2685091]
["ANAMET-M",2685110]
["ANAMET-M",2685111]
["ANAMET-M",2685130]
["ANAMET-M",2685131]
["ANAMET-M",2685160]
["ANAMET-M",2685210]
["ANAMET-M",2685290]
["ANAMET-M",2685360]
["ANAMET-M",2685480]
["ANAMET-M",2686090]
["ANAMET-M",2686110]
["ANAMET-M",2686130]
["ANAMET-M",2686160]
["ANAMET-M",2686210]
["ANAMET-M",2686290]
["ANAMET-M",2686360]
["ANAMET-M",2686480]
["ANAMET-M",2687090]
["ANAMET-M",2687110]
["ANAMET-M",2687130]
["ANAMET-M",2687160]
["ANAMET-M",2687210]
["ANAMET-M",2687290]
["ANAMET-M",2687360]
["ANAMET-M",2687480]
["ANAMET-M",2688070]
["ANAMET-M",2688100]
["ANAMET-M",2688120]
["ANAMET-M",2688130]
["ANAMET-M",2688170]
["ANAMET-M",2688180]
["ANAMET-M",2688230]
["ANAMET-M",2688290]
["ANAMET-M",2688300]
["ANAMET-M",2688370]
["ANAMET-M",2688400]
["ANAMET-M",2688500]
["ANAMET-M",2690703]
["ANAMET-M",2690993]
["ANAMET-M",2691703]
["ANAMET-M",2691993]
["ANAMET-M",2692703]
["ANAMET-M",2692993]
["ANAMET-M",2693703]
["ANAMET-M",2693993]
["ANAMET-M",2699070]
["ANAMET-M",2699073]
["ANAMET-M",2699090]
["ANAMET-M",2699093]
["ANAMET-M",2699110]
["ANAMET-M",2699113]
["ANAMET-M",2699130]
["ANAMET-M",2699133]
["ANAMET-M",2699160]
["ANAMET-M",2699163]
["ANAMET-M",2699210]
["ANAMET-M",2699213]
["ANAMET-M",2699290]
["ANAMET-M",2699293]
["ANAMET-M",2699360]
["ANAMET-M",2699363]
["ANAMET-M",2699480]
["ANAMET-M",2699483]
["ANAMET-S",2930400]
["ANAMET-S",2930407]
["ANAMET-S",2930500]
["ANAMET-S",2930507]
["ANAMET-S",2940630]
["ANAMET-S",2940637]
["ANAMET-S",2940750]
["ANAMET-S",2940757]
["ANAMET-S",2940990]
["ANAMET-S",2940997]
["ANAMET-S",2949630]
["ANAMET-S",2949750]
["ANAMET-S",2949990]
["ANAMET-M",2950120]
["ANAMET-M",2950160]
["ANAMET-M",2950200]
["ANAMET-M",2950260]
["ANAMET-M",2954120]
["ANAMET-M",2954160]
["ANAMET-M",2954200]
["ANAMET-M",2954260]
["ANAMET-M",2959120]
["ANAMET-M",2959160]
["ANAMET-M",2959200]
["ANAMET-M",2959260]
["ANAMET-M",2960120]
["ANAMET-M",2960160]
["ANAMET-M",2960200]
["ANAMET-M",2960260]
["ANAMET-M",2960350]
["ANAMET-M",2960400]
["ANAMET-M",2960500]
["ANAMET-M",2961125]
["ANAMET-M",2961165]
["ANAMET-M",2961205]
["ANAMET-M",2962160]
["ANAMET-M",2962200]
["ANAMET-M",2964120]
["ANAMET-M",2969120]
["ANAMET-M",2969160]
["ANAMET-M",2969200]
["ANAMET-M",2969260]
["ANAMET-M",2969350]
["ANAMET-M",2969400]
["ANAMET-M",2969500]
["ANAMET-M",2970160]
["ANAMET-M",2970200]
["ANAMET-M",2970260]
["ANAMET-M",2970350]
["ANAMET-M",2970400]
["ANAMET-M",2970500]
["ANAMET-M",2972120]
["ANAMET-M",2972160]
["ANAMET-M",2972200]
["ANAMET-M",2972260]
["ANAMET-M",2972350]
["ANAMET-M",2972400]
["ANAMET-M",2972500]
["ANAMET-M",2972630]
["ANAMET-M",2972750]
["ANAMET-S",2972990]
["ANAMET-M",2973120]
["ANAMET-M",2973160]
["ANAMET-M",2973200]
["ANAMET-M",2973260]
["ANAMET-M",2973350]
["ANAMET-M",2973400]
["ANAMET-M",2973500]
["ANAMET-M",2974160]
["ANAMET-M",2974200]
["ANAMET-M",2974260]
["ANAMET-M",2974350]
["ANAMET-M",2974400]
["ANAMET-M",2974500]
["ANAMET-S",2974630]
["ANAMET-S",2974750]
["ANAMET-S",2974990]
["ANAMET-M",2975120]
["ANAMET-M",2975160]
["ANAMET-M",2975200]
["ANAMET-M",2975260]
["ANAMET-M",2975350]
["ANAMET-S",2975400]
["ANAMET-S",2975500]
["ANAMET-M",2976110]
["ANAMET-M",2976120]
["ANAMET-M",2976130]
["ANAMET-M",2976140]
["ANAMET-M",2976150]
["ANAMET-M",2976180]
["ANAMET-M",2976190]
["ANAMET-M",2976230]
["ANAMET-M",2976240]
["ANAMET-M",2976250]
["ANAMET-M",2976290]
["ANAMET-M",2976300]
["ANAMET-M",2976310]
["ANAMET-S",2976430]
["ANAMET-S",2976440]
["ANAMET-S",2976510]
["ANAMET-S",2976520]
["ANAMET-S",2976530]
["ANAMET-M",2978120]
["ANAMET-M",2978129]
["ANAMET-M",2978130]
["ANAMET-M",2978139]
["ANAMET-M",2978140]
["ANAMET-M",2978149]
["ANAMET-M",2978150]
["ANAMET-M",2978159]
["ANAMET-M",2978180]
["ANAMET-M",2978189]
["ANAMET-M",2978190]
["ANAMET-M",2978199]
["ANAMET-M",2978230]
["ANAMET-M",2978239]
["ANAMET-M",2978240]
["ANAMET-M",2978249]
["ANAMET-M",2978250]
["ANAMET-M",2978259]
["ANAMET-M",2978290]
["ANAMET-M",2978299]
["ANAMET-M",2978300]
["ANAMET-M",2978309]
["ANAMET-M",2978310]
["ANAMET-M",2978319]
["ANAMET-S",2978430]
["ANAMET-S",2978439]
["ANAMET-S",2978440]
["ANAMET-S",2978449]
["ANAMET-S",2978510]
["ANAMET-S",2978519]
["ANAMET-S",2978520]
["ANAMET-S",2978529]
["ANAMET-S",2978530]
["ANAMET-S",2978539]
["ANAMET-S",2978540]
["ANAMET-S",2978550]
["ANAMET-S",2978560]
["ANAMET-M",2979120]
["ANAMET-M",2979130]
["ANAMET-M",2979140]
["ANAMET-M",2979150]
["ANAMET-M",2979180]
["ANAMET-M",2979190]
["ANAMET-M",2979230]
["ANAMET-M",2979240]
["ANAMET-M",2979250]
["ANAMET-M",2979290]
["ANAMET-M",2979300]
["ANAMET-M",2979310]
["ANAMET-S",2979430]
["ANAMET-S",2979440]
["ANAMET-S",2979510]
["ANAMET-S",2979520]
["ANAMET-S",2979530]
["ANAMET-S",2979540]
["ANAMET-S",2979550]
["ANAMET-S",2979560]
["ANAMET-M",2980120]
["ANAMET-M",2980126]
["ANAMET-M",2980160]
["ANAMET-M",2980166]
["ANAMET-M",2980200]
["ANAMET-M",2980206]
["ANAMET-M",2980260]
["ANAMET-M",2980266]
["ANAMET-M",2980350]
["ANAMET-M",2980356]
["ANAMET-S",2980400]
["ANAMET-S",2980406]
["ANAMET-S",2980500]
["ANAMET-S",2980506]
["ANAMET-S",2980630]
["ANAMET-S",2980750]
["ANAMET-S",2980990]
["ANAMET-M",2982120]
["ANAMET-M",2982160]
["ANAMET-M",2982200]
["ANAMET-M",2982260]
["ANAMET-M",2982350]
["ANAMET-S",2982400]
["ANAMET-S",2982500]
["ANAMET-M",2983120]
["ANAMET-M",2983160]
["ANAMET-M",2983200]
["ANAMET-M",2983260]
["ANAMET-M",2983350]
["ANAMET-S",2983400]
["ANAMET-S",2983500]
["ANAMET-M",2984120]
["ANAMET-M",2984160]
["ANAMET-M",2984200]
["ANAMET-M",2984260]
["ANAMET-M",2984350]
["ANAMET-S",2984400]
["ANAMET-S",2984500]
["ANAMET-S",2984630]
["ANAMET-S",2984750]
["ANAMET-S",2984990]
["ANAMET-M",2986120]
["ANAMET-M",2986160]
["ANAMET-M",2986200]
["ANAMET-M",2986260]
["ANAMET-M",2987120]
["ANAMET-M",2987160]
["ANAMET-M",2987200]
["ANAMET-M",2987260]
["ANAMET-M",2987350]
["ANAMET-S",2987400]
["ANAMET-S",2987500]
["ANAMET-M",2988120]
["ANAMET-M",2988160]
["ANAMET-M",2988200]
["ANAMET-M",2988260]
["ANAMET-M",2989120]
["ANAMET-M",2989126]
["ANAMET-M",2989160]
["ANAMET-M",2989166]
["ANAMET-M",2989200]
["ANAMET-M",2989206]
["ANAMET-M",2989260]
["ANAMET-M",2989266]
["ANAMET-M",2989350]
["ANAMET-M",2989356]
["ANAMET-S",2989400]
["ANAMET-S",2989406]
["ANAMET-S",2989500]
["ANAMET-S",2989506]
["ANAMET-S",2989630]
["ANAMET-S",2989750]
["ANAMET-S",2989990]
["ANAMET-M",2990110]
["ANAMET-M",2990130]
["ANAMET-M",2990160]
["ANAMET-M",2990200]
["ANAMET-M",2990260]
["ANAMET-M",2990350]
["ANAMET-S",2990400]
["ANAMET-S",2990500]
["ANAMET-M",2994110]
["ANAMET-M",2994130]
["ANAMET-M",2994160]
["ANAMET-M",2994200]
["ANAMET-M",2994260]
["ANAMET-M",2994350]
["ANAMET-S",2994400]
["ANAMET-S",2994500]
["ANAMET-M",2999110]
["ANAMET-M",2999130]
["ANAMET-M",2999160]
["ANAMET-M",2999200]
["ANAMET-M",2999260]
["ANAMET-S",2999400]
["ANAMET-S",2999500]
["ANAMET-S",3000120]
["ANAMET-S",3000160]
["ANAMET-S",3000200]
["ANAMET-S",3000260]
["ANAMET-S",3000350]
["ANAMET-S",3000400]
["ANAMET-S",3000500]
["ANAMET-S",3010701]
["ANAMET-S",3010703]
["ANAMET-S",3010991]
["ANAMET-S",3010993]
["ANAMET-S",3011701]
["ANAMET-S",3011703]
["ANAMET-S",3011991]
["ANAMET-S",3011993]
["ANAMET-S",3012701]
["ANAMET-S",3012703]
["ANAMET-S",3012991]
["ANAMET-S",3012993]
["ANAMET-S",3013701]
["ANAMET-S",3013703]
["ANAMET-S",3013991]
["ANAMET-S",3013993]
["ANAMET-S",3040121]
["ANAMET-S",3040125]
["ANAMET-S",3040161]
["ANAMET-S",3040165]
["ANAMET-S",3040201]
["ANAMET-S",3040203]
["ANAMET-S",3040205]
["ANAMET-S",3040261]
["ANAMET-S",3040265]
["ANAMET-S",3040351]
["ANAMET-S",3040355]
["ANAMET-S",3040401]
["ANAMET-S",3040405]
["ANAMET-S",3040501]
["ANAMET-S",3040505]
["ANAMET-S",3042121]
["ANAMET-S",3042161]
["ANAMET-S",3042201]
["ANAMET-S",3042261]
["ANAMET-S",3042351]
["ANAMET-S",3042401]
["ANAMET-S",3042501]
["ANAMET-S",3090061]
["ANAMET-S",3090101]
["ANAMET-S",3090103]
["ANAMET-S",3090121]
["ANAMET-S",3090123]
["ANAMET-S",3090125]
["ANAMET-S",3090161]
["ANAMET-S",3090163]
["ANAMET-S",3090165]
["ANAMET-S",3090201]
["ANAMET-S",3090203]
["ANAMET-S",3090205]
["ANAMET-S",3090261]
["ANAMET-S",3090263]
["ANAMET-S",3090265]
["ANAMET-S",3090351]
["ANAMET-S",3090355]
["ANAMET-S",3090401]
["ANAMET-S",3090405]
["ANAMET-S",3090501]
["ANAMET-S",3090505]
["ANAMET-S",3100101]
["ANAMET-S",3100121]
["ANAMET-S",3100125]
["ANAMET-S",3100161]
["ANAMET-S",3100165]
["ANAMET-S",3100201]
["ANAMET-S",3100205]
["ANAMET-S",3100261]
["ANAMET-S",3100265]
["ANAMET-S",3100351]
["ANAMET-S",3100355]
["ANAMET-S",3100401]
["ANAMET-S",3100405]
["ANAMET-S",3100501]
["ANAMET-S",3100505]
["ANAMET-S",3110061]
["ANAMET-S",3110101]
["ANAMET-S",3110103]
["ANAMET-S",3110121]
["ANAMET-S",3110123]
["ANAMET-S",3110125]
["ANAMET-S",3110161]
["ANAMET-S",3110163]
["ANAMET-S",3110165]
["ANAMET-S",3110201]
["ANAMET-S",3110203]
["ANAMET-S",3110205]
["ANAMET-S",3110261]
["ANAMET-S",3110263]
["ANAMET-S",3110265]
["ANAMET-S",3110351]
["ANAMET-S",3110353]
["ANAMET-S",3110355]
["ANAMET-S",3110401]
["ANAMET-S",3110405]
["ANAMET-S",3110501]
["ANAMET-S",3110505]
["ANAMET-S",3110631]
["ANAMET-S",3110751]
["ANAMET-S",3111001]
["ANAMET-S",3111251]
["ANAMET-S",3111501]
["ANAMET-S",3125121]
["ANAMET-S",3125161]
["ANAMET-S",3125201]
["ANAMET-S",3125261]
["ANAMET-S",3125351]
["ANAMET-S",3125401]
["ANAMET-S",3125501]
["ANAMET-S",3130121]
["ANAMET-S",3130161]
["ANAMET-S",3130201]
["ANAMET-S",3130261]
["ANAMET-S",3130351]
["ANAMET-S",3130401]
["ANAMET-S",3130501]
["ANAMET-S",3140101]
["ANAMET-S",3140121]
["ANAMET-S",3140125]
["ANAMET-S",3140161]
["ANAMET-S",3140165]
["ANAMET-S",3140201]
["ANAMET-S",3140205]
["ANAMET-S",3140261]
["ANAMET-S",3140265]
["ANAMET-S",3140351]
["ANAMET-S",3140355]
["ANAMET-S",3140401]
["ANAMET-S",3140405]
["ANAMET-S",3140501]
["ANAMET-S",3140505]
["ANAMET-S",3150061]
["ANAMET-S",3150101]
["ANAMET-S",3150103]
["ANAMET-S",3150121]
["ANAMET-S",3150123]
["ANAMET-S",3150125]
["ANAMET-S",3150161]
["ANAMET-S",3150163]
["ANAMET-S",3150165]
["ANAMET-S",3150201]
["ANAMET-S",3150203]
["ANAMET-S",3150205]
["ANAMET-S",3150261]
["ANAMET-S",3150263]
["ANAMET-S",3150265]
["ANAMET-S",3150351]
["ANAMET-S",3150353]
["ANAMET-S",3150355]
["ANAMET-S",3150401]
["ANAMET-S",3150405]
["ANAMET-S",3150501]
["ANAMET-S",3150505]
["ANAMET-S",3150631]
["ANAMET-S",3150751]
["ANAMET-S",3151001]
["ANAMET-S",3151251]
["ANAMET-S",3151501]
["ANAMET-S",3170061]
["ANAMET-S",3170101]
["ANAMET-S",3170103]
["ANAMET-S",3170121]
["ANAMET-S",3170123]
["ANAMET-S",3170125]
["ANAMET-S",3170161]
["ANAMET-S",3170163]
["ANAMET-S",3170165]
["ANAMET-S",3170201]
["ANAMET-S",3170203]
["ANAMET-S",3170205]
["ANAMET-S",3170261]
["ANAMET-S",3170263]
["ANAMET-S",3170265]
["ANAMET-S",3170351]
["ANAMET-S",3170353]
["ANAMET-S",3170355]
["ANAMET-S",3170401]
["ANAMET-S",3170405]
["ANAMET-S",3170501]
["ANAMET-S",3170505]
["ANAMET-S",3180061]
["ANAMET-S",3180101]
["ANAMET-S",3180103]
["ANAMET-S",3180121]
["ANAMET-S",3180123]
["ANAMET-S",3180161]
["ANAMET-S",3180163]
["ANAMET-S",3180201]
["ANAMET-S",3180203]
["ANAMET-S",3180261]
["ANAMET-S",3180263]
["ANAMET-S",3180351]
["ANAMET-S",3180353]
["ANAMET-S",3180401]
["ANAMET-S",3180501]
["ANAMET-S",3190121]
["ANAMET-S",3190123]
["ANAMET-S",3190161]
["ANAMET-S",3190163]
["ANAMET-S",3190201]
["ANAMET-S",3190203]
["ANAMET-S",3190261]
["ANAMET-S",3190263]
["ANAMET-S",3200061]
["ANAMET-S",3200101]
["ANAMET-S",3200103]
["ANAMET-S",3200121]
["ANAMET-S",3200123]
["ANAMET-S",3200125]
["ANAMET-S",3200161]
["ANAMET-S",3200163]
["ANAMET-S",3200165]
["ANAMET-S",3200201]
["ANAMET-S",3200203]
["ANAMET-S",3200205]
["ANAMET-S",3200261]
["ANAMET-S",3200263]
["ANAMET-S",3200265]
["ANAMET-S",3200351]
["ANAMET-S",3200353]
["ANAMET-S",3200355]
["ANAMET-S",3200401]
["ANAMET-S",3200405]
["ANAMET-S",3200501]
["ANAMET-S",3200505]
["ANAMET-S",3200631]
["ANAMET-S",3200751]
["ANAMET-S",3201001]
["ANAMET-S",3210121]
["ANAMET-S",3210161]
["ANAMET-S",3210201]
["ANAMET-S",3210261]
["ANAMET-S",3210351]
["ANAMET-S",3210401]
["ANAMET-S",3210501]
["ANAMET-S",3220121]
["ANAMET-S",3220161]
["ANAMET-S",3220201]
["ANAMET-S",3220261]
["ANAMET-S",3220351]
["ANAMET-S",3230161]
["ANAMET-S",3230201]
["ANAMET-S",3230261]
["ANAMET-S",3230351]
["ANAMET-S",3230401]
["ANAMET-S",3230501]
["ANAMET-S",3240121]
["ANAMET-S",3240161]
["ANAMET-S",3240201]
["ANAMET-S",3240261]
["ANAMET-S",3240351]
["ANAMET-S",3240401]
["ANAMET-S",3240501]
["ANAMET-S",3250120]
["ANAMET-S",3250160]
["ANAMET-S",3250200]
["ANAMET-S",3250260]
["ANAMET-S",3250350]
["ANAMET-S",3250400]
["ANAMET-S",3250500]
["ANAMET-S",3260121]
["ANAMET-S",3260123]
["ANAMET-S",3260125]
["ANAMET-S",3260161]
["ANAMET-S",3260163]
["ANAMET-S",3260165]
["ANAMET-S",3260201]
["ANAMET-S",3260203]
["ANAMET-S",3260205]
["ANAMET-S",3260261]
["ANAMET-S",3260263]
["ANAMET-S",3260265]
["ANAMET-S",3260351]
["ANAMET-S",3260355]
["ANAMET-S",3260401]
["ANAMET-S",3260405]
["ANAMET-S",3260501]
["ANAMET-S",3260505]
["ANAMET-S",3280121]
["ANAMET-S",3280161]
["ANAMET-S",3280201]
["ANAMET-S",3280261]
["ANAMET-S",3280351]
["ANAMET-S",3280401]
["ANAMET-S",3280501]
["ANAMET-S",3300122]
["ANAMET-S",3300123]
["ANAMET-S",3300125]
["ANAMET-S",3300162]
["ANAMET-S",3300163]
["ANAMET-S",3300165]
["ANAMET-S",3300202]
["ANAMET-S",3300203]
["ANAMET-S",3300205]
["ANAMET-S",3300261]
["ANAMET-S",3300263]
["ANAMET-S",3300265]
["ANAMET-S",3300351]
["ANAMET-S",3300355]
["ANAMET-S",3300401]
["ANAMET-S",3300405]
["ANAMET-S",3300501]
["ANAMET-S",3300505]
["ANAMET-S",3310061]
["ANAMET-S",3310101]
["ANAMET-S",3310103]
["ANAMET-S",3310121]
["ANAMET-S",3310123]
["ANAMET-S",3310125]
["ANAMET-S",3310161]
["ANAMET-S",3310163]
["ANAMET-S",3310165]
["ANAMET-S",3310201]
["ANAMET-S",3310203]
["ANAMET-S",3310205]
["ANAMET-S",3310261]
["ANAMET-S",3310263]
["ANAMET-S",3310265]
["ANAMET-S",3310351]
["ANAMET-S",3310355]
["ANAMET-S",3310401]
["ANAMET-S",3310501]
["ANAMET-S",3320121]
["ANAMET-S",3320161]
["ANAMET-S",3320201]
["ANAMET-S",3320261]
["ANAMET-S",3320351]
["ANAMET-S",3320401]
["ANAMET-S",3320501]
["ANAMET-S",3330061]
["ANAMET-S",3330101]
["ANAMET-S",3330103]
["ANAMET-S",3330121]
["ANAMET-S",3330123]
["ANAMET-S",3330161]
["ANAMET-S",3330163]
["ANAMET-S",3330201]
["ANAMET-S",3330203]
["ANAMET-S",3330261]
["ANAMET-S",3330263]
["ANAMET-S",3330351]
["ANAMET-S",3340121]
["ANAMET-S",3340125]
["ANAMET-S",3340161]
["ANAMET-S",3340165]
["ANAMET-S",3340201]
["ANAMET-S",3340205]
["ANAMET-S",3340261]
["ANAMET-S",3340265]
["ANAMET-S",3340351]
["ANAMET-S",3340355]
["ANAMET-S",3340401]
["ANAMET-S",3340405]
["ANAMET-S",3340501]
["ANAMET-S",3340505]
["ANAMET-S",3352121]
["ANAMET-S",3352161]
["ANAMET-S",3352201]
["ANAMET-S",3352261]
["ANAMET-S",3352351]
["ANAMET-S",3352401]
["ANAMET-S",3352501]
["ANAMET-S",3360060]
["ANAMET-S",3360061]
["ANAMET-S",3360063]
["ANAMET-S",3360100]
["ANAMET-S",3360101]
["ANAMET-S",3360103]
["ANAMET-S",3360131]
["ANAMET-S",3360133]
["ANAMET-S",3360160]
["ANAMET-S",3360161]
["ANAMET-S",3360163]
["ANAMET-S",3360190]
["ANAMET-S",3360191]
["ANAMET-S",3360193]
["ANAMET-S",3360220]
["ANAMET-S",3360221]
["ANAMET-S",3360223]
["ANAMET-S",3360250]
["ANAMET-S",3360251]
["ANAMET-S",3360253]
["ANAMET-S",3360290]
["ANAMET-S",3360291]
["ANAMET-S",3360293]
["ANAMET-S",3360320]
["ANAMET-S",3360321]
["ANAMET-S",3360323]
["ANAMET-S",3360350]
["ANAMET-S",3360351]
["ANAMET-S",3360353]
["ANAMET-S",3360380]
["ANAMET-S",3360381]
["ANAMET-S",3360383]
["ANAMET-S",3360410]
["ANAMET-S",3360411]
["ANAMET-S",3360413]
["ANAMET-S",3360440]
["ANAMET-S",3360441]
["ANAMET-S",3360443]
["ANAMET-S",3360510]
["ANAMET-S",3360511]
["ANAMET-S",3360513]
["ANAMET-S",3360571]
["ANAMET-S",3360573]
["ANAMET-S",3360641]
["ANAMET-S",3360643]
["ANAMET-S",3360701]
["ANAMET-S",3360703]
["ANAMET-S",3360761]
["ANAMET-S",3360763]
["ANAMET-S",3360831]
["ANAMET-S",3360833]
["ANAMET-S",3360891]
["ANAMET-S",3360893]
["ANAMET-S",3360951]
["ANAMET-S",3360953]
["ANAMET-S",3361021]
["ANAMET-S",3361023]
["ANAMET-S",3363400]
["ANAMET-S",3363401]
["ANAMET-S",3363405]
["ANAMET-S",3363500]
["ANAMET-S",3363501]
["ANAMET-S",3363505]
["ANAMET-S",3364200]
["ANAMET-S",3364201]
["ANAMET-S",3364205]
["ANAMET-S",3364400]
["ANAMET-S",3364401]
["ANAMET-S",3364405]
["ANAMET-S",3364700]
["ANAMET-S",3364701]
["ANAMET-S",3364703]
["ANAMET-S",3365250]
["ANAMET-S",3365251]
["ANAMET-S",3365256]
["ANAMET-S",3365320]
["ANAMET-S",3365321]
["ANAMET-S",3365326]
["ANAMET-S",3365380]
["ANAMET-S",3365381]
["ANAMET-S",3365386]
["ANAMET-S",3365440]
["ANAMET-S",3365441]
["ANAMET-S",3365446]
["ANAMET-S",3365510]
["ANAMET-S",3365511]
["ANAMET-S",3365516]
["ANAMET-S",3365570]
["ANAMET-S",3365571]
["ANAMET-S",3365576]
["ANAMET-S",3365640]
["ANAMET-S",3365641]
["ANAMET-S",3365646]
["ANAMET-S",3365700]
["ANAMET-S",3365701]
["ANAMET-S",3365706]
["ANAMET-S",3365760]
["ANAMET-S",3365761]
["ANAMET-S",3365766]
["ANAMET-S",3365830]
["ANAMET-S",3365831]
["ANAMET-S",3365836]
["ANAMET-S",3365890]
["ANAMET-S",3365891]
["ANAMET-S",3365896]
["ANAMET-S",3365950]
["ANAMET-S",3365951]
["ANAMET-S",3365956]
["ANAMET-S",3366041]
["ANAMET-S",3366043]
["ANAMET-S",3366048]
["ANAMET-S",3366061]
["ANAMET-S",3366063]
["ANAMET-S",3366068]
["ANAMET-S",3366101]
["ANAMET-S",3366103]
["ANAMET-S",3366108]
["ANAMET-S",3366141]
["ANAMET-S",3366143]
["ANAMET-S",3366148]
["ANAMET-S",3366221]
["ANAMET-S",3366223]
["ANAMET-S",3366228]
["ANAMET-S",3366441]
["ANAMET-S",3366443]
["ANAMET-S",3368063]
["ANAMET-S",3368103]
["ANAMET-S",3368133]
["ANAMET-S",3368163]
["ANAMET-S",3368193]
["ANAMET-S",3368223]
["ANAMET-S",3368253]
["ANAMET-S",3368293]
["ANAMET-S",3368323]
["ANAMET-S",3368353]
["ANAMET-S",3368383]
["ANAMET-S",3368413]
["ANAMET-S",3368443]
["ANAMET-S",3368513]
["ANAMET-S",3368573]
["ANAMET-S",3368643]
["ANAMET-S",3368703]
["ANAMET-S",3368763]
["ANAMET-S",3368833]
["ANAMET-S",3368893]
["ANAMET-S",3368953]
["ANAMET-S",3368973]
["ANAMET-S",3368981]
["ANAMET-S",3368983]
["ANAMET-S",3368991]
["ANAMET-S",3368993]
["ANAMET-S",3369400]
["ANAMET-S",3369401]
["ANAMET-S",3369406]
["ANAMET-S",3369450]
["ANAMET-S",3369451]
["ANAMET-S",3369456]
["ANAMET-S",3369500]
["ANAMET-S",3369501]
["ANAMET-S",3369506]
["ANAMET-S",3369550]
["ANAMET-S",3369551]
["ANAMET-S",3369556]
["ANAMET-S",3369600]
["ANAMET-S",3369601]
["ANAMET-S",3369606]
["ANAMET-S",3369650]
["ANAMET-S",3369651]
["ANAMET-S",3369656]
["ANAMET-S",3369700]
["ANAMET-S",3369701]
["ANAMET-S",3369706]
["ANAMET-S",3369750]
["ANAMET-S",3369751]
["ANAMET-S",3369756]
["ANAMET-S",3369800]
["ANAMET-S",3369801]
["ANAMET-S",3369806]
["ANAMET-S",3369850]
["ANAMET-S",3369851]
["ANAMET-S",3369856]
["ANAMET-S",3369900]
["ANAMET-S",3369901]
["ANAMET-S",3369906]
["ANAMET-S",3369910]
["ANAMET-S",3369911]
["ANAMET-S",3369916]
["ANAMET-S",3369920]
["ANAMET-S",3369921]
["ANAMET-S",3369926]
["ANAMET-S",3369940]
["ANAMET-S",3369941]
["ANAMET-S",3369946]
["ANAMET-S",3369960]
["ANAMET-S",3369961]
["ANAMET-S",3369966]
["ANAMET-S",3370251]
["ANAMET-S",3370253]
["ANAMET-S",3370501]
["ANAMET-S",3370503]
["ANAMET-S",3370761]
["ANAMET-S",3370763]
["ANAMET-S",3371001]
["ANAMET-S",3371003]
["ANAMET-S",3371271]
["ANAMET-S",3371273]
["ANAMET-S",3374251]
["ANAMET-S",3374381]
["ANAMET-S",3375251]
["ANAMET-S",3375381]
["ANAMET-S",3376251]
["ANAMET-S",3376253]
["ANAMET-S",3376501]
["ANAMET-S",3376503]
["ANAMET-S",3376761]
["ANAMET-S",3376763]
["ANAMET-S",3376991]
["ANAMET-S",3376993]
["ANAMET-S",3377250]
["ANAMET-S",3377253]
["ANAMET-S",3377380]
["ANAMET-S",3377383]
["ANAMET-S",3377510]
["ANAMET-S",3377513]
["ANAMET-S",3377640]
["ANAMET-S",3377643]
["ANAMET-S",3377760]
["ANAMET-S",3377763]
["ANAMET-S",3377890]
["ANAMET-S",3377893]
["ANAMET-S",3377990]
["ANAMET-S",3377991]
["ANAMET-S",3392121]
["ANAMET-S",3392161]
["ANAMET-S",3392201]
["ANAMET-S",3392261]
["ANAMET-S",3392351]
["ANAMET-S",3400121]
["ANAMET-S",3400123]
["ANAMET-S",3400161]
["ANAMET-S",3400163]
["ANAMET-S",3400201]
["ANAMET-S",3400203]
["ANAMET-S",3400261]
["ANAMET-S",3400263]
["ANAMET-S",3400351]
["ANAMET-S",3410121]
["ANAMET-S",3410161]
["ANAMET-S",3410201]
["ANAMET-S",3410261]
["ANAMET-S",3410351]
["ANAMET-S",3410401]
["ANAMET-S",3410501]
["ANAMET-S",3460133]
["ANAMET-S",3460163]
["ANAMET-S",3460193]
["ANAMET-S",3460293]
["ANAMET-S",3460353]
["ANAMET-S",3460413]
["ANAMET-S",3460513]
["ANAMET-S",3461133]
["ANAMET-S",3461163]
["ANAMET-S",3461193]
["ANAMET-S",3461293]
["ANAMET-S",3461353]
["ANAMET-S",3461413]
["ANAMET-S",3461513]
["ANAMET-S",3462133]
["ANAMET-S",3462163]
["ANAMET-S",3462193]
["ANAMET-S",3462293]
["ANAMET-S",3462353]
["ANAMET-S",3462413]
["ANAMET-S",3462513]
["ANAMET-S",3463133]
["ANAMET-S",3463163]
["ANAMET-S",3463193]
["ANAMET-S",3463293]
["ANAMET-S",3463353]
["ANAMET-S",3463383]
["ANAMET-S",3463413]
["ANAMET-S",3463513]
["ANAMET-S",3469133]
["ANAMET-S",3469163]
["ANAMET-S",3469193]
["ANAMET-S",3469293]
["ANAMET-S",3469353]
["ANAMET-S",3469383]
["ANAMET-S",3469413]
["ANAMET-S",3469511]
["ANAMET-S",3470161]
["ANAMET-S",3470241]
["ANAMET-S",3470321]
["ANAMET-S",3470481]
["ANAMET-S",3470641]
["ANAMET-S",3474200]
["ANAMET-S",3474205]
["ANAMET-S",3474300]
["ANAMET-S",3474305]
["ANAMET-S",3480101]
["ANAMET-S",3480121]
["ANAMET-S",3480161]
["ANAMET-S",3480201]
["ANAMET-S",3480261]
["ANAMET-S",3480351]
["ANAMET-S",3480401]
["ANAMET-S",3480501]
["ANAMET-S",3500121]
["ANAMET-S",3500161]
["ANAMET-S",3500201]
["ANAMET-S",3500261]
["ANAMET-S",3500351]
["ANAMET-S",3500401]
["ANAMET-S",3500501]
["ANAMET-S",3520121]
["ANAMET-S",3520161]
["ANAMET-S",3520201]
["ANAMET-S",3520261]
["ANAMET-S",3520351]
["ANAMET-S",3520401]
["ANAMET-S",3520501]
["ANAMET-S",3550045]
["ANAMET-S",3550065]
["ANAMET-S",3550085]
["ANAMET-S",3550105]
["ANAMET-S",3550125]
["ANAMET-S",3550165]
["ANAMET-S",3550205]
["ANAMET-S",3567323]
["ANAMET-S",3567383]
["ANAMET-S",3567513]
["ANAMET-S",3567763]
["ANAMET-S",3567993]
["ANAMET-S",3571028]
["ANAMET-S",3571048]
["ANAMET-S",3571058]
["ANAMET-S",3571068]
["ANAMET-S",3571088]
["ANAMET-S",3571108]
["ANAMET-S",3571128]
["ANAMET-S",3571168]
["ANAMET-S",3571188]
["ANAMET-S",3571228]
["ANAMET-S",3580121]
["ANAMET-S",3580161]
["ANAMET-S",3580201]
["ANAMET-S",3580261]
["ANAMET-S",3580351]
["ANAMET-S",3590120]
["ANAMET-S",3590160]
["ANAMET-S",3590200]
["ANAMET-S",3590260]
["ANAMET-S",3590350]
["ANAMET-S",3590400]
["ANAMET-S",3590500]
["ANAMET-S",3600105]
["ANAMET-S",3600121]
["ANAMET-S",3600125]
["ANAMET-S",3600161]
["ANAMET-S",3600165]
["ANAMET-S",3600181]
["ANAMET-S",3600185]
["ANAMET-S",3600201]
["ANAMET-S",3600205]
["ANAMET-S",3600251]
["ANAMET-S",3600255]
["ANAMET-S",3600321]
["ANAMET-S",3600322]
["ANAMET-S",3600401]
["ANAMET-S",3600402]
["ANAMET-S",3600501]
["ANAMET-S",3600502]
["ANAMET-S",3610105]
["ANAMET-S",3610121]
["ANAMET-S",3610125]
["ANAMET-S",3610161]
["ANAMET-S",3610165]
["ANAMET-S",3610181]
["ANAMET-S",3610185]
["ANAMET-S",3610201]
["ANAMET-S",3610205]
["ANAMET-S",3610251]
["ANAMET-S",3610255]
["ANAMET-S",3610321]
["ANAMET-S",3610322]
["ANAMET-S",3610401]
["ANAMET-S",3610402]
["ANAMET-S",3610501]
["ANAMET-S",3610502]
["ANAMET-S",3700122]
["ANAMET-S",3700125]
["ANAMET-S",3700161]
["ANAMET-S",3700162]
["ANAMET-S",3700165]
["ANAMET-S",3700201]
["ANAMET-S",3700202]
["ANAMET-S",3700205]
["ANAMET-S",3700251]
["ANAMET-S",3700252]
["ANAMET-S",3700255]
["ANAMET-S",3700321]
["ANAMET-S",3700322]
["ANAMET-S",3700401]
["ANAMET-S",3700402]
["ANAMET-S",3700501]
["ANAMET-S",3700502]
["ANAMET-S",3710102]
["ANAMET-S",3710105]
["ANAMET-S",3710122]
["ANAMET-S",3710125]
["ANAMET-S",3710161]
["ANAMET-S",3710162]
["ANAMET-S",3710165]
["ANAMET-S",3710201]
["ANAMET-S",3710202]
["ANAMET-S",3710205]
["ANAMET-S",3710251]
["ANAMET-S",3710252]
["ANAMET-S",3710255]
["ANAMET-S",3710321]
["ANAMET-S",3710322]
["ANAMET-S",3710401]
["ANAMET-S",3710402]
["ANAMET-S",3710501]
["ANAMET-S",3710502]
["ANAMET-S",3720125]
["ANAMET-S",3720161]
["ANAMET-S",3720165]
["ANAMET-S",3720201]
["ANAMET-S",3720205]
["ANAMET-S",3720251]
["ANAMET-S",3720255]
["ANAMET-S",3720321]
["ANAMET-S",3720322]
["ANAMET-S",3720401]
["ANAMET-S",3720501]
["ANAMET-S",3730122]
["ANAMET-S",3730162]
["ANAMET-S",3730165]
["ANAMET-S",3730201]
["ANAMET-S",3730202]
["ANAMET-S",3730205]
["ANAMET-S",3730251]
["ANAMET-S",3730252]
["ANAMET-S",3730255]
["ANAMET-S",3730321]
["ANAMET-S",3730322]
["ANAMET-S",3730401]
["ANAMET-S",3730402]
["ANAMET-S",3730501]
["ANAMET-S",3730502]
["ANAMET-S",3740122]
["ANAMET-S",3740162]
["ANAMET-S",3740202]
["ANAMET-S",3740252]
["ANAMET-S",3740322]
["ANAMET-S",3740401]
["ANAMET-S",3740501]
["ANAMET-S",4650121]
["ANAMET-S",4650123]
["ANAMET-S",4650125]
["ANAMET-S",4650161]
["ANAMET-S",4650163]
["ANAMET-S",4650165]
["ANAMET-S",4650201]
["ANAMET-S",4650203]
["ANAMET-S",4650205]
["ANAMET-S",5110100]
["ANAMET-S",5120100]
["ANAMET-S",5120120]
["ANAMET-S",5120160]
["ANAMET-S",5120220]
["ANAMET-S",5120250]
["ANAMET-S",5120340]
["ANAMET-S",5120400]
["ANAMET-S",5120500]
["ANAMET-S",5150100]
["ANAMET-S",5150120]
["ANAMET-S",5150160]
["ANAMET-S",5150220]
["ANAMET-S",5150250]
["ANAMET-S",5150340]
["ANAMET-S",5150400]
["ANAMET-S",5150500]
["ANAMET-S",5150630]
["ANAMET-S",5150750]
["ANAMET-S",5150990]
["ANAMET-S",5750300]
["ANAMET-S",5750400]
["ANAMET-S",5750450]
["ANAMET-S",5750600]
["ANAMET-S",5751450]
["ANAMET-S",5758400]
["ANAMET-S",6000032]
["ANAMET-S",6000042]
["ANAMET-S",6000052]
["ANAMET-S",6000062]
["ANAMET-S",6000072]
["ANAMET-S",6000082]
["ANAMET-S",6000102]
["ANAMET-S",6000122]
["ANAMET-S",6000162]
["ANAMET-S",6000202]
["ANAMET-S",6000262]
["ANAMET-S",6000352]
["ANAMET-S",6006102]
["ANAMET-S",6006122]
["ANAMET-S",6006162]
["ANAMET-S",6006202]
["ANAMET-S",6006262]
["ANAMET-S",6006352]
["ANAMET-S",6203090]
["ANAMET-S",6203091]
["ANAMET-S",6203110]
["ANAMET-S",6203111]
["ANAMET-S",6203130]
["ANAMET-S",6203131]
["ANAMET-S",6203160]
["ANAMET-S",6203161]
["ANAMET-S",6203210]
["ANAMET-S",6203211]
["ANAMET-S",6203290]
["ANAMET-S",6203291]
["ANAMET-S",6203360]
["ANAMET-S",6203361]
["ANAMET-S",6203420]
["ANAMET-S",6203421]
["ANAMET-S",6203480]
["ANAMET-S",6203481]
["ANAMET-S",6204090]
["ANAMET-S",6204091]
["ANAMET-S",6204110]
["ANAMET-S",6204111]
["ANAMET-S",6204130]
["ANAMET-S",6204131]
["ANAMET-S",6204160]
["ANAMET-S",6204161]
["ANAMET-S",6204210]
["ANAMET-S",6204211]
["ANAMET-S",6204290]
["ANAMET-S",6204291]
["ANAMET-S",6204360]
["ANAMET-S",6204361]
["ANAMET-S",6204420]
["ANAMET-S",6204421]
["ANAMET-S",6204480]
["ANAMET-S",6204481]
["ANAMET-M",6505092]
["ANAMET-M",6505112]
["ANAMET-M",6505132]
["ANAMET-M",6505162]
["ANAMET-M",6505212]
["ANAMET-M",6505292]
["ANAMET-M",6505362]
["ANAMET-M",6505422]
["ANAMET-M",6505482]
["ANAMET-M",6506093]
["ANAMET-M",6506113]
["ANAMET-M",6506133]
["ANAMET-M",6506163]
["ANAMET-M",6506213]
["ANAMET-M",6506293]
["ANAMET-M",6507092]
["ANAMET-M",6507112]
["ANAMET-M",6507132]
["ANAMET-M",6507162]
["ANAMET-M",6507212]
["ANAMET-M",6507292]
["ANAMET-M",6507362]
["ANAMET-M",6507422]
["ANAMET-M",6507482]
["ANAMET-M",6508094]
["ANAMET-M",6508114]
["ANAMET-M",6508134]
["ANAMET-M",6508164]
["ANAMET-M",6508214]
["ANAMET-M",6508294]
["ANAMET-M",6508364]
["ANAMET-M",6508424]
["ANAMET-M",6508484]
["ANAMET-M",6513162]
["ANAMET-M",6513202]
["ANAMET-M",6513252]
["ANAMET-M",6513322]
["ANAMET-M",6513402]
["ANAMET-M",6513502]
["ANAMET-M",6513632]
["ANAMET-M",6517162]
["ANAMET-M",6517172]
["ANAMET-M",6517202]
["ANAMET-M",6517252]
["ANAMET-M",6517322]
["ANAMET-M",6517402]
["ANAMET-M",6517502]
["ANAMET-M",6517632]
["ANAMET-M",6518124]
["ANAMET-M",6518164]
["ANAMET-M",6518174]
["ANAMET-M",6518204]
["ANAMET-M",6518254]
["ANAMET-M",6518324]
["ANAMET-M",6518404]
["ANAMET-M",6518504]
["ANAMET-M",6518634]
["ANAMET-M",7100111]
["ANAMET-M",7100114]
["ANAMET-M",7100115]
["ANAMET-M",7100116]
["ANAMET-M",7100117]
["ANAMET-M",7100131]
["ANAMET-M",7100134]
["ANAMET-M",7100135]
["ANAMET-M",7100136]
["ANAMET-M",7100137]
["ANAMET-M",7100161]
["ANAMET-M",7100164]
["ANAMET-M",7100165]
["ANAMET-M",7100166]
["ANAMET-M",7100167]
["ANAMET-M",7100211]
["ANAMET-M",7100214]
["ANAMET-M",7100215]
["ANAMET-M",7100216]
["ANAMET-M",7100217]
["ANAMET-M",7100291]
["ANAMET-M",7100294]
["ANAMET-M",7100295]
["ANAMET-M",7100296]
["ANAMET-M",7100297]
["ANAMET-M",7100361]
["ANAMET-M",7100366]
["ANAMET-M",7100367]
["ANAMET-S",7100404]
["ANAMET-M",7100421]
["ANAMET-M",7100427]
["ANAMET-S",7100454]
["ANAMET-M",7100481]
["ANAMET-M",7100487]
["ANAMET-S",7100504]
["ANAMET-M",7109111]
["ANAMET-M",7109114]
["ANAMET-M",7109115]
["ANAMET-M",7109116]
["ANAMET-M",7109117]
["ANAMET-M",7109131]
["ANAMET-M",7109134]
["ANAMET-M",7109135]
["ANAMET-M",7109136]
["ANAMET-M",7109137]
["ANAMET-M",7109161]
["ANAMET-M",7109164]
["ANAMET-M",7109165]
["ANAMET-M",7109166]
["ANAMET-M",7109167]
["ANAMET-M",7109211]
["ANAMET-M",7109214]
["ANAMET-M",7109215]
["ANAMET-M",7109216]
["ANAMET-M",7109217]
["ANAMET-M",7109291]
["ANAMET-M",7109294]
["ANAMET-M",7109295]
["ANAMET-M",7109296]
["ANAMET-M",7109297]
["ANAMET-M",7109361]
["ANAMET-M",7109366]
["ANAMET-M",7109367]
["ANAMET-S",7109404]
["ANAMET-M",7109421]
["ANAMET-M",7109427]
["ANAMET-S",7109454]
["ANAMET-M",7109481]
["ANAMET-M",7109487]
["ANAMET-S",7109504]
["ANAMET-M",7120140]
["ANAMET-M",7120143]
["ANAMET-M",7120144]
["ANAMET-M",7120146]
["ANAMET-M",7120147]
["ANAMET-M",7120149]
["ANAMET-M",7120150]
["ANAMET-M",7120153]
["ANAMET-M",7120154]
["ANAMET-M",7120156]
["ANAMET-M",7120157]
["ANAMET-M",7120159]
["ANAMET-M",7120161]
["ANAMET-M",7120163]
["ANAMET-M",7120164]
["ANAMET-M",7120165]
["ANAMET-M",7120166]
["ANAMET-M",7120167]
["ANAMET-M",7120168]
["ANAMET-M",7120169]
["ANAMET-M",7120171]
["ANAMET-M",7120173]
["ANAMET-M",7120174]
["ANAMET-M",7120175]
["ANAMET-M",7120176]
["ANAMET-M",7120177]
["ANAMET-M",7120178]
["ANAMET-M",7120179]
["ANAMET-M",7120201]
["ANAMET-M",7120203]
["ANAMET-M",7120204]
["ANAMET-M",7120205]
["ANAMET-M",7120206]
["ANAMET-M",7120207]
["ANAMET-M",7120208]
["ANAMET-M",7120209]
["ANAMET-M",7120251]
["ANAMET-M",7120253]
["ANAMET-M",7120254]
["ANAMET-M",7120255]
["ANAMET-M",7120256]
["ANAMET-M",7120257]
["ANAMET-M",7120258]
["ANAMET-M",7120259]
["ANAMET-M",7120321]
["ANAMET-M",7120323]
["ANAMET-M",7120324]
["ANAMET-M",7120325]
["ANAMET-M",7120326]
["ANAMET-M",7120327]
["ANAMET-M",7120328]
["ANAMET-M",7120329]
["ANAMET-M",7120401]
["ANAMET-M",7120404]
["ANAMET-M",7120405]
["ANAMET-M",7120406]
["ANAMET-M",7120407]
["ANAMET-M",7120408]
["ANAMET-M",7120409]
["ANAMET-S",7120454]
["ANAMET-M",7120501]
["ANAMET-M",7120507]
["ANAMET-M",7120508]
["ANAMET-M",7120509]
["ANAMET-S",7120554]
["ANAMET-S",7120604]
["ANAMET-M",7120631]
["ANAMET-M",7120637]
["ANAMET-M",7120638]
["ANAMET-M",7120639]
["ANAMET-M",7121149]
["ANAMET-M",7121159]
["ANAMET-M",7121168]
["ANAMET-M",7121169]
["ANAMET-M",7121178]
["ANAMET-M",7121179]
["ANAMET-M",7121208]
["ANAMET-M",7121209]
["ANAMET-M",7121258]
["ANAMET-M",7121259]
["ANAMET-M",7121328]
["ANAMET-M",7121329]
["ANAMET-M",7121408]
["ANAMET-M",7121409]
["ANAMET-M",7121508]
["ANAMET-M",7121509]
["ANAMET-M",7121638]
["ANAMET-M",7121639]
["ANAMET-M",7124140]
["ANAMET-M",7124150]
["ANAMET-M",7124161]
["ANAMET-M",7124171]
["ANAMET-M",7124201]
["ANAMET-M",7124251]
["ANAMET-M",7124321]
["ANAMET-M",7125169]
["ANAMET-M",7125179]
["ANAMET-M",7125209]
["ANAMET-M",7125259]
["ANAMET-M",7125329]
["ANAMET-M",7125409]
["ANAMET-M",7125509]
["ANAMET-M",7125639]
["ANAMET-M",7129140]
["ANAMET-M",7129144]
["ANAMET-M",7129146]
["ANAMET-M",7129147]
["ANAMET-M",7129150]
["ANAMET-M",7129154]
["ANAMET-M",7129156]
["ANAMET-M",7129157]
["ANAMET-M",7129161]
["ANAMET-M",7129164]
["ANAMET-M",7129165]
["ANAMET-M",7129166]
["ANAMET-M",7129167]
["ANAMET-M",7129168]
["ANAMET-M",7129169]
["ANAMET-M",7129171]
["ANAMET-M",7129174]
["ANAMET-M",7129175]
["ANAMET-M",7129176]
["ANAMET-M",7129177]
["ANAMET-M",7129178]
["ANAMET-M",7129179]
["ANAMET-M",7129201]
["ANAMET-M",7129204]
["ANAMET-M",7129205]
["ANAMET-M",7129206]
["ANAMET-M",7129207]
["ANAMET-M",7129208]
["ANAMET-M",7129209]
["ANAMET-M",7129251]
["ANAMET-M",7129254]
["ANAMET-M",7129255]
["ANAMET-M",7129256]
["ANAMET-M",7129257]
["ANAMET-M",7129258]
["ANAMET-M",7129259]
["ANAMET-M",7129321]
["ANAMET-M",7129324]
["ANAMET-M",7129325]
["ANAMET-M",7129326]
["ANAMET-M",7129327]
["ANAMET-M",7129328]
["ANAMET-M",7129329]
["ANAMET-M",7129401]
["ANAMET-M",7129406]
["ANAMET-M",7129407]
["ANAMET-M",7129408]
["ANAMET-M",7129409]
["ANAMET-S",7129454]
["ANAMET-M",7129501]
["ANAMET-M",7129507]
["ANAMET-M",7129508]
["ANAMET-M",7129509]
["ANAMET-S",7129554]
["ANAMET-S",7129604]
["ANAMET-M",7129631]
["ANAMET-M",7129637]
["ANAMET-M",7129638]
["ANAMET-M",7129639]
["ANAMET-M",7140121]
["ANAMET-M",7140122]
["ANAMET-M",7140124]
["ANAMET-M",7140125]
["ANAMET-M",7140126]
["ANAMET-M",7140127]
["ANAMET-M",7140128]
["ANAMET-M",7140129]
["ANAMET-M",7140161]
["ANAMET-M",7140162]
["ANAMET-M",7140164]
["ANAMET-M",7140165]
["ANAMET-M",7140166]
["ANAMET-M",7140167]
["ANAMET-M",7140168]
["ANAMET-M",7140169]
["ANAMET-M",7140201]
["ANAMET-M",7140202]
["ANAMET-M",7140204]
["ANAMET-M",7140205]
["ANAMET-M",7140206]
["ANAMET-M",7140207]
["ANAMET-M",7140208]
["ANAMET-M",7140209]
["ANAMET-M",7140261]
["ANAMET-M",7140262]
["ANAMET-M",7140264]
["ANAMET-M",7140265]
["ANAMET-M",7140266]
["ANAMET-M",7140267]
["ANAMET-M",7140268]
["ANAMET-M",7140269]
["ANAMET-M",7140351]
["ANAMET-M",7140352]
["ANAMET-S",7140354]
["ANAMET-M",7140356]
["ANAMET-M",7140357]
["ANAMET-M",7140358]
["ANAMET-M",7140359]
["ANAMET-M",7140401]
["ANAMET-M",7140402]
["ANAMET-M",7140407]
["ANAMET-M",7140408]
["ANAMET-M",7140409]
["ANAMET-S",7140454]
["ANAMET-M",7140501]
["ANAMET-M",7140502]
["ANAMET-M",7140507]
["ANAMET-M",7140508]
["ANAMET-M",7140509]
["ANAMET-S",7140554]
["ANAMET-M",7141128]
["ANAMET-M",7141129]
["ANAMET-M",7141168]
["ANAMET-M",7141169]
["ANAMET-M",7141208]
["ANAMET-M",7141209]
["ANAMET-M",7141268]
["ANAMET-M",7141269]
["ANAMET-M",7141358]
["ANAMET-M",7141359]
["ANAMET-M",7141408]
["ANAMET-M",7141409]
["ANAMET-M",7141508]
["ANAMET-M",7141509]
["ANAMET-M",7144121]
["ANAMET-M",7144161]
["ANAMET-M",7144201]
["ANAMET-M",7144261]
["ANAMET-M",7145129]
["ANAMET-M",7145169]
["ANAMET-M",7145209]
["ANAMET-M",7145269]
["ANAMET-M",7145359]
["ANAMET-M",7145409]
["ANAMET-M",7145509]
["ANAMET-M",7149121]
["ANAMET-M",7149122]
["ANAMET-M",7149124]
["ANAMET-M",7149125]
["ANAMET-M",7149126]
["ANAMET-M",7149127]
["ANAMET-M",7149128]
["ANAMET-M",7149129]
["ANAMET-M",7149161]
["ANAMET-M",7149162]
["ANAMET-M",7149164]
["ANAMET-M",7149165]
["ANAMET-M",7149166]
["ANAMET-M",7149167]
["ANAMET-M",7149168]
["ANAMET-M",7149169]
["ANAMET-M",7149201]
["ANAMET-M",7149202]
["ANAMET-M",7149204]
["ANAMET-M",7149205]
["ANAMET-M",7149206]
["ANAMET-M",7149207]
["ANAMET-M",7149208]
["ANAMET-M",7149209]
["ANAMET-M",7149261]
["ANAMET-M",7149262]
["ANAMET-M",7149264]
["ANAMET-M",7149265]
["ANAMET-M",7149266]
["ANAMET-M",7149267]
["ANAMET-M",7149268]
["ANAMET-M",7149269]
["ANAMET-M",7149351]
["ANAMET-M",7149352]
["ANAMET-S",7149354]
["ANAMET-M",7149356]
["ANAMET-M",7149357]
["ANAMET-M",7149358]
["ANAMET-M",7149359]
["ANAMET-M",7149401]
["ANAMET-M",7149402]
["ANAMET-M",7149407]
["ANAMET-M",7149408]
["ANAMET-M",7149409]
["ANAMET-S",7149454]
["ANAMET-M",7149501]
["ANAMET-M",7149502]
["ANAMET-M",7149507]
["ANAMET-M",7149508]
["ANAMET-M",7149509]
["ANAMET-S",7149554]
["ANAMET-S",7189400]
["ANAMET-S",7189500]
["ANAMET-S",7189630]
["ANAMET-M",7811110]
["ANAMET-M",7811150]
["ANAMET-M",7811160]
["ANAMET-M",7811180]
["ANAMET-M",7811210]
["ANAMET-S",7811290]
["ANAMET-S",7811360]
["ANAMET-S",7811480]
["ANAMET-M",7812200]
["ANAMET-M",7812250]
["ANAMET-M",7812320]
["ANAMET-S",7812400]
["ANAMET-S",7812500]
["ANAMET-S",7812630]
["ANAMET-M",7813160]
["ANAMET-M",7813200]
["ANAMET-M",7813250]
["ANAMET-M",7813320]
["ANAMET-S",7813400]
["ANAMET-S",7813500]
["ANAMET-S",7813630]
["ANAMET-S",7813750]
["ANAMET-M",7814160]
["ANAMET-M",7814200]
["ANAMET-M",7814260]
["ANAMET-S",7814350]
["ANAMET-S",7814400]
["ANAMET-S",7814500]
["ANAMET-M",7815110]
["ANAMET-M",7815130]
["ANAMET-M",7815160]
["ANAMET-M",7815210]
["ANAMET-M",7815290]
["ANAMET-S",7815360]
["ANAMET-S",7815480]
["ANAMET-M",7817160]
["ANAMET-M",7817200]
["ANAMET-M",7817260]
["ANAMET-S",7817350]
["ANAMET-S",7817400]
["ANAMET-S",7817500]
["ANAMET-M",7821110]
["ANAMET-M",7821160]
["ANAMET-M",7821210]
["ANAMET-M",7821290]
["ANAMET-S",7821360]
["ANAMET-M",7822160]
["ANAMET-M",7822200]
["ANAMET-M",7822250]
["ANAMET-M",7822320]
["ANAMET-S",7822400]
["ANAMET-S",7822500]
["ANAMET-M",7823110]
["ANAMET-M",7823130]
["ANAMET-M",7823160]
["ANAMET-M",7823200]
["ANAMET-M",7823210]
["ANAMET-M",7823260]
["ANAMET-M",7823290]
["ANAMET-S",7823300]
["ANAMET-S",7823360]
["ANAMET-S",7823400]
["ANAMET-S",7823420]
["ANAMET-S",7823480]
["ANAMET-M",7824110]
["ANAMET-M",7824120]
["ANAMET-M",7824130]
["ANAMET-M",7824160]
["ANAMET-M",7824200]
["ANAMET-M",7824260]
["ANAMET-S",7824350]
["ANAMET-S",7824400]
["ANAMET-S",7824500]
["ANAMET-M",7825160]
["ANAMET-M",7825200]
["ANAMET-M",7825220]
["ANAMET-M",7825240]
["ANAMET-M",7825250]
["ANAMET-M",7825270]
["ANAMET-M",7825280]
["ANAMET-M",7825320]
["ANAMET-S",7825340]
["ANAMET-S",7825380]
["ANAMET-S",7825400]
["ANAMET-S",7825480]
["ANAMET-S",7825500]
["ANAMET-S",7825520]
["ANAMET-S",7825600]
["ANAMET-S",7825630]
["ANAMET-M",7826120]
["ANAMET-M",7826160]
["ANAMET-M",7826180]
["ANAMET-M",7826200]
["ANAMET-M",7826260]
["ANAMET-S",7826350]
["ANAMET-S",7826400]
["ANAMET-S",7826500]
["ANAMET-M",7827160]
["ANAMET-M",7827200]
["ANAMET-M",7827260]
["ANAMET-S",7827350]
["ANAMET-S",7827400]
["ANAMET-S",7827500]
["ANAMET-M",7829160]
["ANAMET-M",7829200]
["ANAMET-M",7829250]
["ANAMET-M",7829320]
["ANAMET-S",7829400]
["ANAMET-S",7829500]
["ANAMET-S",7829630]
["ANAMET-M",7830160]
["ANAMET-M",7830200]
["ANAMET-M",7830250]
["ANAMET-M",7830320]
["ANAMET-M",7840100]
["ANAMET-M",7840104]
["ANAMET-M",7840106]
["ANAMET-M",7840107]
["ANAMET-M",7840120]
["ANAMET-M",7840124]
["ANAMET-M",7840125]
["ANAMET-M",7840126]
["ANAMET-M",7840127]
["ANAMET-M",7840160]
["ANAMET-M",7840164]
["ANAMET-M",7840165]
["ANAMET-M",7840166]
["ANAMET-M",7840167]
["ANAMET-M",7840200]
["ANAMET-M",7840204]
["ANAMET-M",7840205]
["ANAMET-M",7840206]
["ANAMET-M",7840207]
["ANAMET-M",7840260]
["ANAMET-M",7840264]
["ANAMET-M",7840265]
["ANAMET-M",7840266]
["ANAMET-M",7840267]
["ANAMET-M",7840350]
["ANAMET-S",7840354]
["ANAMET-M",7840356]
["ANAMET-M",7840357]
["ANAMET-M",7840400]
["ANAMET-M",7840407]
["ANAMET-S",7840454]
["ANAMET-M",7840500]
["ANAMET-M",7840507]
["ANAMET-M",7852340]
["ANAMET-M",7852350]
["ANAMET-M",7852430]
["ANAMET-M",7852440]
["ANAMET-M",7853270]
["ANAMET-M",7853366]
["ANAMET-M",7853380]
["ANAMET-M",7854375]
["ANAMET-M",7854480]
["ANAMET-M",7854650]
["ANAMET-M",7854660]
["ANAMET-M",7977010]
["ANAMET-M",7977020]
["ANAMET-M",7977030]
["ANAMET-M",7977040]
["ANAMET-M",7977050]
["ANAMET-M",7977060]
["ANAMET-M",7977070]
["ANAMET-M",7977080]
["ANAMET-M",7977090]
["ANAMET-M",7977100]
["ANAMET-M",7977110]
["ANAMET-M",7977120]
["ANAMET-M",7977130]
["ANAMET-M",7977140]
["ANAMET-M",7977150]
["ANAMET-M",7978010]
["ANAMET-M",7978020]
["ANAMET-M",7978030]
["ANAMET-M",7978040]
["ANAMET-M",7978050]
["ANAMET-M",7978060]
["ANAMET-M",7978070]
["ANAMET-M",7978080]
["ANAMET-M",7978090]
["ANAMET-M",7978100]
["ANAMET-M",7978110]
["ANAMET-M",7983120]
["ANAMET-M",7983123]
["ANAMET-M",7983160]
["ANAMET-M",7983163]
["ANAMET-M",7983200]
["ANAMET-M",7983203]
["ANAMET-M",7983250]
["ANAMET-M",7983253]
["ANAMET-M",7983320]
["ANAMET-M",7983323]
["ANAMET-M",7983400]
["ANAMET-M",7983403]
["ANAMET-M",7983500]
["ANAMET-M",7983503]
["ANAMET-M",7983630]
["ANAMET-M",7983633]
["ANAMET-M",7998010]
["ANAMET-M",7998020]
["ANAMET-M",7998030]
["ANAMET-M",7998040]
["ANAMET-M",7998050]
["ANAMET-M",7998060]
["ANAMET-M",7998070]
["ANAMET-S",8011070]
["ANAMET-S",8011075]
["ANAMET-S",8011100]
["ANAMET-S",8011105]
["ANAMET-S",8011120]
["ANAMET-S",8011125]
["ANAMET-S",8011170]
["ANAMET-S",8011175]
["ANAMET-S",8011230]
["ANAMET-S",8011235]
["ANAMET-S",8011290]
["ANAMET-S",8011295]
["ANAMET-S",8011360]
["ANAMET-S",8011365]
["ANAMET-S",8011480]
["ANAMET-S",8011485]
["ANAMET-S",8012070]
["ANAMET-S",8012075]
["ANAMET-S",8012100]
["ANAMET-S",8012105]
["ANAMET-S",8012120]
["ANAMET-S",8012125]
["ANAMET-S",8012170]
["ANAMET-S",8012175]
["ANAMET-S",8012230]
["ANAMET-S",8012235]
["ANAMET-S",8012290]
["ANAMET-S",8012295]
["ANAMET-S",8012360]
["ANAMET-S",8012365]
["ANAMET-S",8012480]
["ANAMET-S",8012485]
["ANAMET-S",8013050]
["ANAMET-S",8013055]
["ANAMET-S",8013070]
["ANAMET-S",8013075]
["ANAMET-S",8013100]
["ANAMET-S",8013105]
["ANAMET-S",8013120]
["ANAMET-S",8013125]
["ANAMET-S",8013170]
["ANAMET-S",8013175]
["ANAMET-S",8013230]
["ANAMET-S",8013235]
["ANAMET-S",8013290]
["ANAMET-S",8013295]
["ANAMET-S",8013360]
["ANAMET-S",8013365]
["ANAMET-S",8013480]
["ANAMET-S",8013485]
["ANAMET-S",8015070]
["ANAMET-S",8015075]
["ANAMET-S",8015100]
["ANAMET-S",8015105]
["ANAMET-S",8015120]
["ANAMET-S",8015125]
["ANAMET-S",8015170]
["ANAMET-S",8015175]
["ANAMET-S",8015230]
["ANAMET-S",8015235]
["ANAMET-S",8015290]
["ANAMET-S",8015295]
["ANAMET-S",8015360]
["ANAMET-S",8015365]
["ANAMET-S",8017070]
["ANAMET-S",8017100]
["ANAMET-S",8017120]
["ANAMET-S",8017170]
["ANAMET-S",8017230]
["ANAMET-S",8017290]
["ANAMET-S",8017360]
["ANAMET-S",8017480]
["ANAMET-S",8022070]
["ANAMET-S",8022100]
["ANAMET-S",8022130]
["ANAMET-S",8022160]
["ANAMET-S",8022170]
["ANAMET-S",8022220]
["ANAMET-S",8022230]
["ANAMET-S",8022260]
["ANAMET-S",8022290]
["ANAMET-S",8022360]
["ANAMET-S",8022480]
["ANAMET-S",8023070]
["ANAMET-S",8023100]
["ANAMET-S",8023130]
["ANAMET-S",8023160]
["ANAMET-S",8023170]
["ANAMET-S",8023220]
["ANAMET-S",8023230]
["ANAMET-S",8023260]
["ANAMET-S",8023290]
["ANAMET-S",8023360]
["ANAMET-S",8023480]
["ANAMET-S",8025100]
["ANAMET-S",8025120]
["ANAMET-S",8025170]
["ANAMET-S",8025230]
["ANAMET-S",8025290]
["ANAMET-S",8025360]
["ANAMET-S",8025480]
["ANAMET-S",8028050]
["ANAMET-S",8028055]
["ANAMET-S",8028060]
["ANAMET-S",8028065]
["ANAMET-S",8028070]
["ANAMET-S",8028075]
["ANAMET-S",8028100]
["ANAMET-S",8028105]
["ANAMET-S",8028120]
["ANAMET-S",8028125]
["ANAMET-S",8028140]
["ANAMET-S",8028145]
["ANAMET-S",8028170]
["ANAMET-S",8028175]
["ANAMET-S",8028190]
["ANAMET-S",8028195]
["ANAMET-S",8028230]
["ANAMET-S",8028235]
["ANAMET-S",8028260]
["ANAMET-S",8028265]
["ANAMET-S",8028290]
["ANAMET-S",8028295]
["ANAMET-S",8028360]
["ANAMET-S",8028365]
["ANAMET-S",8028480]
["ANAMET-S",8028485]
["ANAMET-S",8029070]
["ANAMET-S",8029100]
["ANAMET-S",8029130]
["ANAMET-S",8029160]
["ANAMET-S",8029170]
["ANAMET-S",8029220]
["ANAMET-S",8029230]
["ANAMET-S",8029260]
["ANAMET-S",8029290]
["ANAMET-S",8029360]
["ANAMET-S",8029480]
["ANAMET-M",8100071]
["ANAMET-M",8100072]
["ANAMET-M",8100091]
["ANAMET-M",8100092]
["ANAMET-M",8100096]
["ANAMET-M",8100097]
["ANAMET-M",8100101]
["ANAMET-M",8100106]
["ANAMET-M",8100107]
["ANAMET-M",8100111]
["ANAMET-M",8100116]
["ANAMET-M",8100117]
["ANAMET-M",8100118]
["ANAMET-M",8100119]
["ANAMET-M",8100121]
["ANAMET-M",8100126]
["ANAMET-M",8100127]
["ANAMET-M",8100128]
["ANAMET-M",8100129]
["ANAMET-M",8100131]
["ANAMET-M",8100136]
["ANAMET-M",8100137]
["ANAMET-M",8100139]
["ANAMET-M",8100141]
["ANAMET-M",8100149]
["ANAMET-M",8100161]
["ANAMET-M",8100166]
["ANAMET-M",8100167]
["ANAMET-M",8100168]
["ANAMET-M",8100169]
["ANAMET-M",8100210]
["ANAMET-M",8100211]
["ANAMET-M",8100216]
["ANAMET-M",8100217]
["ANAMET-M",8100218]
["ANAMET-M",8100219]
["ANAMET-M",8100291]
["ANAMET-M",8100296]
["ANAMET-M",8100297]
["ANAMET-M",8100299]
["ANAMET-M",8100361]
["ANAMET-M",8100366]
["ANAMET-M",8100367]
["ANAMET-M",8100369]
["ANAMET-M",8100421]
["ANAMET-M",8100427]
["ANAMET-M",8100429]
["ANAMET-M",8100481]
["ANAMET-M",8100487]
["ANAMET-M",8100489]
["ANAMET-M",8101169]
["ANAMET-M",8101219]
["ANAMET-M",8101299]
["ANAMET-M",8103032]
["ANAMET-M",8103036]
["ANAMET-M",8103037]
["ANAMET-M",8103041]
["ANAMET-M",8103045]
["ANAMET-M",8103046]
["ANAMET-M",8103047]
["ANAMET-M",8103111]
["ANAMET-M",8103115]
["ANAMET-M",8103116]
["ANAMET-M",8103117]
["ANAMET-M",8103121]
["ANAMET-M",8103126]
["ANAMET-M",8103127]
["ANAMET-M",8103131]
["ANAMET-M",8103135]
["ANAMET-M",8103136]
["ANAMET-M",8103137]
["ANAMET-M",8103141]
["ANAMET-M",8103146]
["ANAMET-M",8103161]
["ANAMET-M",8103165]
["ANAMET-M",8103166]
["ANAMET-M",8103167]
["ANAMET-M",8103211]
["ANAMET-M",8103215]
["ANAMET-M",8103216]
["ANAMET-M",8103217]
["ANAMET-M",8103291]
["ANAMET-M",8103295]
["ANAMET-M",8103296]
["ANAMET-M",8103297]
["ANAMET-M",8103361]
["ANAMET-M",8103366]
["ANAMET-M",8103367]
["ANAMET-M",8103421]
["ANAMET-M",8103427]
["ANAMET-M",8103481]
["ANAMET-M",8103487]
["ANAMET-M",8104111]
["ANAMET-M",8104121]
["ANAMET-M",8104131]
["ANAMET-M",8104141]
["ANAMET-M",8104161]
["ANAMET-M",8104211]
["ANAMET-M",8104291]
["ANAMET-S",8104361]
["ANAMET-S",8104421]
["ANAMET-S",8104481]
["ANAMET-M",8106091]
["ANAMET-M",8106111]
["ANAMET-M",8106121]
["ANAMET-M",8106151]
["ANAMET-M",8106161]
["ANAMET-M",8106211]
["ANAMET-M",8106291]
["ANAMET-M",8107091]
["ANAMET-M",8107096]
["ANAMET-M",8107097]
["ANAMET-M",8107111]
["ANAMET-M",8107115]
["ANAMET-M",8107116]
["ANAMET-M",8107117]
["ANAMET-M",8107121]
["ANAMET-M",8107126]
["ANAMET-M",8107127]
["ANAMET-M",8107146]
["ANAMET-M",8107151]
["ANAMET-M",8107155]
["ANAMET-M",8107156]
["ANAMET-M",8107157]
["ANAMET-M",8107161]
["ANAMET-M",8107165]
["ANAMET-M",8107166]
["ANAMET-M",8107167]
["ANAMET-M",8107211]
["ANAMET-M",8107215]
["ANAMET-M",8107216]
["ANAMET-M",8107217]
["ANAMET-M",8107291]
["ANAMET-M",8107295]
["ANAMET-M",8107296]
["ANAMET-M",8107297]
["ANAMET-M",8109111]
["ANAMET-M",8109118]
["ANAMET-M",8109119]
["ANAMET-M",8109121]
["ANAMET-M",8109128]
["ANAMET-M",8109129]
["ANAMET-M",8109131]
["ANAMET-M",8109141]
["ANAMET-M",8109161]
["ANAMET-M",8109168]
["ANAMET-M",8109169]
["ANAMET-M",8109211]
["ANAMET-M",8109218]
["ANAMET-M",8109219]
["ANAMET-M",8109291]
["ANAMET-M",8109299]
["ANAMET-S",8109361]
["ANAMET-S",8109421]
["ANAMET-S",8109481]
["ANAMET-M",8120112]
["ANAMET-M",8120121]
["ANAMET-M",8120122]
["ANAMET-M",8120125]
["ANAMET-M",8120132]
["ANAMET-M",8120141]
["ANAMET-M",8120142]
["ANAMET-M",8120146]
["ANAMET-M",8120147]
["ANAMET-M",8120148]
["ANAMET-M",8120149]
["ANAMET-M",8120151]
["ANAMET-M",8120152]
["ANAMET-M",8120156]
["ANAMET-M",8120157]
["ANAMET-M",8120158]
["ANAMET-M",8120159]
["ANAMET-M",8120161]
["ANAMET-M",8120166]
["ANAMET-M",8120167]
["ANAMET-M",8120168]
["ANAMET-M",8120169]
["ANAMET-M",8120171]
["ANAMET-M",8120176]
["ANAMET-M",8120177]
["ANAMET-M",8120178]
["ANAMET-M",8120179]
["ANAMET-M",8120201]
["ANAMET-M",8120206]
["ANAMET-M",8120207]
["ANAMET-M",8120208]
["ANAMET-M",8120209]
["ANAMET-M",8120250]
["ANAMET-M",8120251]
["ANAMET-M",8120256]
["ANAMET-M",8120257]
["ANAMET-M",8120258]
["ANAMET-M",8120259]
["ANAMET-M",8120321]
["ANAMET-M",8120326]
["ANAMET-M",8120327]
["ANAMET-M",8120328]
["ANAMET-M",8120329]
["ANAMET-M",8120401]
["ANAMET-M",8120406]
["ANAMET-M",8120407]
["ANAMET-M",8120408]
["ANAMET-M",8120409]
["ANAMET-M",8120501]
["ANAMET-M",8120507]
["ANAMET-M",8120631]
["ANAMET-M",8120637]
["ANAMET-S",8120751]
["ANAMET-M",8121169]
["ANAMET-M",8121209]
["ANAMET-M",8121259]
["ANAMET-M",8121329]
["ANAMET-M",8123151]
["ANAMET-M",8123156]
["ANAMET-M",8123157]
["ANAMET-M",8123161]
["ANAMET-M",8123165]
["ANAMET-M",8123166]
["ANAMET-M",8123167]
["ANAMET-M",8123201]
["ANAMET-M",8123205]
["ANAMET-M",8123206]
["ANAMET-M",8123207]
["ANAMET-M",8123221]
["ANAMET-M",8123226]
["ANAMET-M",8123227]
["ANAMET-M",8123231]
["ANAMET-M",8123235]
["ANAMET-M",8123236]
["ANAMET-M",8123237]
["ANAMET-M",8123251]
["ANAMET-M",8123255]
["ANAMET-M",8123256]
["ANAMET-M",8123257]
["ANAMET-M",8123261]
["ANAMET-M",8123266]
["ANAMET-M",8123267]
["ANAMET-M",8123271]
["ANAMET-M",8123275]
["ANAMET-M",8123276]
["ANAMET-M",8123277]
["ANAMET-M",8123291]
["ANAMET-M",8123295]
["ANAMET-M",8123296]
["ANAMET-M",8123297]
["ANAMET-M",8123321]
["ANAMET-M",8123325]
["ANAMET-M",8123326]
["ANAMET-M",8123327]
["ANAMET-M",8123381]
["ANAMET-M",8123386]
["ANAMET-M",8123387]
["ANAMET-M",8123401]
["ANAMET-M",8123406]
["ANAMET-M",8123407]
["ANAMET-M",8123421]
["ANAMET-M",8123426]
["ANAMET-M",8123427]
["ANAMET-M",8123501]
["ANAMET-M",8123507]
["ANAMET-M",8123631]
["ANAMET-M",8123637]
["ANAMET-M",8124141]
["ANAMET-M",8124149]
["ANAMET-M",8124151]
["ANAMET-M",8124159]
["ANAMET-M",8124161]
["ANAMET-M",8124169]
["ANAMET-M",8124171]
["ANAMET-M",8124179]
["ANAMET-M",8124201]
["ANAMET-M",8124209]
["ANAMET-M",8124251]
["ANAMET-M",8124259]
["ANAMET-M",8124321]
["ANAMET-S",8124401]
["ANAMET-M",8124501]
["ANAMET-S",8124631]
["ANAMET-M",8126152]
["ANAMET-M",8126157]
["ANAMET-M",8126161]
["ANAMET-M",8126167]
["ANAMET-M",8126171]
["ANAMET-M",8126177]
["ANAMET-M",8126201]
["ANAMET-M",8126207]
["ANAMET-M",8126221]
["ANAMET-M",8126227]
["ANAMET-M",8126281]
["ANAMET-M",8126287]
["ANAMET-M",8126351]
["ANAMET-M",8126357]
["ANAMET-M",8127152]
["ANAMET-M",8127153]
["ANAMET-M",8127156]
["ANAMET-M",8127157]
["ANAMET-M",8127158]
["ANAMET-M",8127159]
["ANAMET-M",8127161]
["ANAMET-M",8127162]
["ANAMET-M",8127163]
["ANAMET-M",8127164]
["ANAMET-M",8127165]
["ANAMET-M",8127166]
["ANAMET-M",8127167]
["ANAMET-M",8127168]
["ANAMET-M",8127169]
["ANAMET-M",8127171]
["ANAMET-M",8127173]
["ANAMET-M",8127174]
["ANAMET-M",8127175]
["ANAMET-M",8127176]
["ANAMET-M",8127177]
["ANAMET-M",8127178]
["ANAMET-M",8127179]
["ANAMET-M",8127201]
["ANAMET-M",8127202]
["ANAMET-M",8127203]
["ANAMET-M",8127204]
["ANAMET-M",8127205]
["ANAMET-M",8127206]
["ANAMET-M",8127207]
["ANAMET-M",8127208]
["ANAMET-M",8127209]
["ANAMET-M",8127221]
["ANAMET-M",8127224]
["ANAMET-M",8127225]
["ANAMET-M",8127252]
["ANAMET-M",8127253]
["ANAMET-M",8127254]
["ANAMET-M",8127255]
["ANAMET-M",8127256]
["ANAMET-M",8127257]
["ANAMET-M",8127281]
["ANAMET-M",8127284]
["ANAMET-M",8127285]
["ANAMET-M",8127322]
["ANAMET-M",8127323]
["ANAMET-M",8127324]
["ANAMET-M",8127325]
["ANAMET-M",8127326]
["ANAMET-M",8127327]
["ANAMET-M",8127351]
["ANAMET-M",8127402]
["ANAMET-M",8127406]
["ANAMET-M",8127407]
["ANAMET-S",8127454]
["ANAMET-M",8127502]
["ANAMET-M",8127507]
["ANAMET-S",8127554]
["ANAMET-S",8127604]
["ANAMET-M",8127632]
["ANAMET-M",8127637]
["ANAMET-M",8129141]
["ANAMET-M",8129149]
["ANAMET-M",8129151]
["ANAMET-M",8129159]
["ANAMET-M",8129161]
["ANAMET-M",8129169]
["ANAMET-M",8129171]
["ANAMET-M",8129179]
["ANAMET-M",8129201]
["ANAMET-M",8129209]
["ANAMET-M",8129251]
["ANAMET-M",8129259]
["ANAMET-M",8129321]
["ANAMET-S",8129401]
["ANAMET-S",8129501]
["ANAMET-S",8129631]
["ANAMET-M",8130150]
["ANAMET-M",8130153]
["ANAMET-M",8130154]
["ANAMET-M",8130156]
["ANAMET-M",8130160]
["ANAMET-M",8130163]
["ANAMET-M",8130164]
["ANAMET-M",8130165]
["ANAMET-M",8130166]
["ANAMET-M",8130167]
["ANAMET-M",8130200]
["ANAMET-M",8130203]
["ANAMET-M",8130204]
["ANAMET-M",8130205]
["ANAMET-M",8130206]
["ANAMET-M",8130207]
["ANAMET-M",8130250]
["ANAMET-M",8130253]
["ANAMET-M",8130254]
["ANAMET-M",8130255]
["ANAMET-M",8130256]
["ANAMET-M",8130257]
["ANAMET-M",8130320]
["ANAMET-M",8130323]
["ANAMET-M",8130324]
["ANAMET-M",8130325]
["ANAMET-M",8130326]
["ANAMET-M",8130327]
["ANAMET-M",8130400]
["ANAMET-M",8130406]
["ANAMET-M",8130407]
["ANAMET-S",8130454]
["ANAMET-M",8130500]
["ANAMET-M",8130507]
["ANAMET-S",8130554]
["ANAMET-S",8130604]
["ANAMET-M",8130630]
["ANAMET-M",8130637]
["ANAMET-M",8134160]
["ANAMET-M",8134200]
["ANAMET-M",8134250]
["ANAMET-M",8134320]
["ANAMET-M",8139150]
["ANAMET-M",8139154]
["ANAMET-M",8139156]
["ANAMET-M",8139157]
["ANAMET-M",8139160]
["ANAMET-M",8139164]
["ANAMET-M",8139165]
["ANAMET-M",8139166]
["ANAMET-M",8139167]
["ANAMET-M",8139200]
["ANAMET-M",8139204]
["ANAMET-M",8139205]
["ANAMET-M",8139206]
["ANAMET-M",8139207]
["ANAMET-M",8139250]
["ANAMET-M",8139254]
["ANAMET-M",8139255]
["ANAMET-M",8139256]
["ANAMET-M",8139257]
["ANAMET-M",8139320]
["ANAMET-M",8139324]
["ANAMET-M",8139325]
["ANAMET-M",8139326]
["ANAMET-M",8139327]
["ANAMET-M",8140111]
["ANAMET-M",8140117]
["ANAMET-M",8140118]
["ANAMET-M",8140119]
["ANAMET-M",8140121]
["ANAMET-M",8140127]
["ANAMET-M",8140128]
["ANAMET-M",8140129]
["ANAMET-M",8140161]
["ANAMET-M",8140167]
["ANAMET-M",8140168]
["ANAMET-M",8140169]
["ANAMET-M",8140201]
["ANAMET-M",8140207]
["ANAMET-M",8140208]
["ANAMET-M",8140209]
["ANAMET-M",8140261]
["ANAMET-M",8140267]
["ANAMET-M",8140268]
["ANAMET-M",8140269]
["ANAMET-M",8140351]
["ANAMET-M",8140357]
["ANAMET-M",8140401]
["ANAMET-M",8140407]
["ANAMET-M",8140501]
["ANAMET-M",8140507]
["ANAMET-M",8141129]
["ANAMET-M",8141169]
["ANAMET-M",8141209]
["ANAMET-M",8141269]
["ANAMET-M",8143111]
["ANAMET-M",8143117]
["ANAMET-M",8143121]
["ANAMET-M",8143125]
["ANAMET-M",8143127]
["ANAMET-M",8143161]
["ANAMET-M",8143165]
["ANAMET-M",8143167]
["ANAMET-M",8143201]
["ANAMET-M",8143205]
["ANAMET-M",8143207]
["ANAMET-M",8143261]
["ANAMET-M",8143265]
["ANAMET-M",8143267]
["ANAMET-M",8143351]
["ANAMET-M",8143357]
["ANAMET-M",8143401]
["ANAMET-M",8143407]
["ANAMET-M",8143501]
["ANAMET-M",8143507]
["ANAMET-M",8144111]
["ANAMET-M",8144119]
["ANAMET-M",8144121]
["ANAMET-M",8144129]
["ANAMET-M",8144161]
["ANAMET-M",8144169]
["ANAMET-M",8144201]
["ANAMET-M",8144209]
["ANAMET-M",8144261]
["ANAMET-S",8144351]
["ANAMET-S",8144401]
["ANAMET-S",8144501]
["ANAMET-M",8145129]
["ANAMET-M",8145169]
["ANAMET-M",8145209]
["ANAMET-M",8147091]
["ANAMET-M",8147097]
["ANAMET-M",8147101]
["ANAMET-M",8147107]
["ANAMET-M",8147121]
["ANAMET-M",8147127]
["ANAMET-M",8147151]
["ANAMET-M",8147157]
["ANAMET-M",8147211]
["ANAMET-M",8147217]
["ANAMET-M",8149111]
["ANAMET-M",8149118]
["ANAMET-M",8149119]
["ANAMET-M",8149121]
["ANAMET-M",8149128]
["ANAMET-M",8149129]
["ANAMET-M",8149161]
["ANAMET-M",8149168]
["ANAMET-M",8149169]
["ANAMET-M",8149201]
["ANAMET-M",8149208]
["ANAMET-M",8149209]
["ANAMET-M",8149261]
["ANAMET-M",8149269]
["ANAMET-S",8149351]
["ANAMET-S",8149401]
["ANAMET-S",8149501]
["ANAMET-M",8150060]
["ANAMET-M",8150100]
["ANAMET-M",8150110]
["ANAMET-M",8150112]
["ANAMET-M",8150113]
["ANAMET-M",8150115]
["ANAMET-M",8150117]
["ANAMET-M",8150119]
["ANAMET-M",8150160]
["ANAMET-M",8150162]
["ANAMET-M",8150163]
["ANAMET-M",8150165]
["ANAMET-M",8150167]
["ANAMET-M",8150169]
["ANAMET-M",8150210]
["ANAMET-M",8150212]
["ANAMET-M",8150213]
["ANAMET-M",8150215]
["ANAMET-M",8150217]
["ANAMET-M",8150219]
["ANAMET-M",8150290]
["ANAMET-M",8150292]
["ANAMET-M",8150293]
["ANAMET-M",8150295]
["ANAMET-M",8150297]
["ANAMET-M",8150299]
["ANAMET-M",8150362]
["ANAMET-M",8150363]
["ANAMET-M",8150365]
["ANAMET-M",8150367]
["ANAMET-M",8150422]
["ANAMET-M",8150423]
["ANAMET-M",8150425]
["ANAMET-M",8150482]
["ANAMET-M",8150483]
["ANAMET-M",8150485]
["ANAMET-M",8154160]
["ANAMET-M",8154200]
["ANAMET-M",8154250]
["ANAMET-M",8154320]
["ANAMET-M",8154400]
["ANAMET-M",8154500]
["ANAMET-M",8154630]
["ANAMET-M",8155070]
["ANAMET-M",8155090]
["ANAMET-M",8155110]
["ANAMET-M",8155130]
["ANAMET-M",8155160]
["ANAMET-M",8155210]
["ANAMET-M",8155290]
["ANAMET-M",8155360]
["ANAMET-M",8155420]
["ANAMET-M",8155480]
["ANAMET-M",8156160]
["ANAMET-M",8156200]
["ANAMET-M",8156260]
["ANAMET-M",8156350]
["ANAMET-M",8156400]
["ANAMET-M",8156500]
["ANAMET-M",8171120]
["ANAMET-M",8171160]
["ANAMET-M",8171200]
["ANAMET-M",8171250]
["ANAMET-M",8171320]
["ANAMET-M",8172066]
["ANAMET-M",8172069]
["ANAMET-M",8172096]
["ANAMET-M",8172099]
["ANAMET-M",8172106]
["ANAMET-M",8172109]
["ANAMET-M",8172136]
["ANAMET-M",8172139]
["ANAMET-M",8172166]
["ANAMET-M",8172169]
["ANAMET-M",8172206]
["ANAMET-M",8172209]
["ANAMET-M",8172266]
["ANAMET-M",8172269]
["ANAMET-M",8172356]
["ANAMET-M",8172359]
["ANAMET-M",8172406]
["ANAMET-M",8172409]
["ANAMET-M",8172506]
["ANAMET-M",8172509]
["ANAMET-S",8172636]
["ANAMET-S",8172756]
["ANAMET-S",8172996]
["ANAMET-M",8173126]
["ANAMET-M",8173166]
["ANAMET-M",8173206]
["ANAMET-M",8173266]
["ANAMET-M",8175120]
["ANAMET-M",8175160]
["ANAMET-M",8175200]
["ANAMET-M",8175260]
["ANAMET-M",8175350]
["ANAMET-M",8175400]
["ANAMET-M",8175500]
["ANAMET-M",8176120]
["ANAMET-M",8176160]
["ANAMET-M",8176200]
["ANAMET-M",8176260]
["ANAMET-M",8176350]
["ANAMET-M",8176400]
["ANAMET-M",8176500]
["ANAMET-M",8177100]
["ANAMET-M",8177120]
["ANAMET-M",8177160]
["ANAMET-M",8177200]
["ANAMET-M",8177260]
["ANAMET-M",8177350]
["ANAMET-M",8177400]
["ANAMET-M",8177500]
["ANAMET-M",8189161]
["ANAMET-M",8189201]
["ANAMET-M",8189251]
["ANAMET-M",8189321]
["ANAMET-S",8189401]
["ANAMET-S",8189501]
["ANAMET-S",8189631]
["ANAMET-M",8192129]
["ANAMET-M",8192169]
["ANAMET-M",8194120]
["ANAMET-M",8194160]
["ANAMET-M",8194200]
["ANAMET-M",8194260]
["ANAMET-M",8195129]
["ANAMET-M",8195169]
["ANAMET-M",8199120]
["ANAMET-M",8199124]
["ANAMET-M",8199160]
["ANAMET-M",8199164]
["ANAMET-M",8199200]
["ANAMET-M",8199204]
["ANAMET-M",8199260]
["ANAMET-M",8199264]
["ANAMET-M",8218120]
["ANAMET-M",8218129]
["ANAMET-M",8218130]
["ANAMET-M",8218139]
["ANAMET-M",8218140]
["ANAMET-M",8218149]
["ANAMET-M",8218150]
["ANAMET-M",8218159]
["ANAMET-M",8218180]
["ANAMET-M",8218189]
["ANAMET-M",8218190]
["ANAMET-M",8218199]
["ANAMET-M",8218230]
["ANAMET-M",8218239]
["ANAMET-M",8218240]
["ANAMET-M",8218249]
["ANAMET-M",8218250]
["ANAMET-M",8218259]
["ANAMET-M",8218290]
["ANAMET-M",8218299]
["ANAMET-M",8218300]
["ANAMET-M",8218309]
["ANAMET-M",8218310]
["ANAMET-M",8218319]
["ANAMET-S",8218430]
["ANAMET-S",8218439]
["ANAMET-S",8218440]
["ANAMET-S",8218449]
["ANAMET-S",8218510]
["ANAMET-S",8218519]
["ANAMET-S",8218520]
["ANAMET-S",8218529]
["ANAMET-S",8218530]
["ANAMET-S",8218539]
["ANAMET-S",8218540]
["ANAMET-S",8218550]
["ANAMET-S",8218560]
["ANAMET-M",8220080]
["ANAMET-M",8220090]
["ANAMET-M",8220093]
["ANAMET-M",8220096]
["ANAMET-M",8220099]
["ANAMET-M",8220100]
["ANAMET-M",8220103]
["ANAMET-M",8220106]
["ANAMET-M",8220109]
["ANAMET-M",8220110]
["ANAMET-M",8220113]
["ANAMET-M",8220116]
["ANAMET-M",8220119]
["ANAMET-M",8220120]
["ANAMET-M",8220123]
["ANAMET-M",8220126]
["ANAMET-M",8220129]
["ANAMET-M",8220130]
["ANAMET-M",8220133]
["ANAMET-M",8220136]
["ANAMET-M",8220139]
["ANAMET-M",8220140]
["ANAMET-M",8220143]
["ANAMET-M",8220146]
["ANAMET-M",8220149]
["ANAMET-M",8220150]
["ANAMET-M",8220153]
["ANAMET-M",8220156]
["ANAMET-M",8220159]
["ANAMET-M",8220180]
["ANAMET-M",8220183]
["ANAMET-M",8220186]
["ANAMET-M",8220189]
["ANAMET-M",8220190]
["ANAMET-M",8220193]
["ANAMET-M",8220196]
["ANAMET-M",8220199]
["ANAMET-M",8220230]
["ANAMET-M",8220233]
["ANAMET-M",8220236]
["ANAMET-M",8220239]
["ANAMET-M",8220240]
["ANAMET-M",8220243]
["ANAMET-M",8220246]
["ANAMET-M",8220249]
["ANAMET-M",8220250]
["ANAMET-M",8220253]
["ANAMET-M",8220256]
["ANAMET-M",8220259]
["ANAMET-M",8220290]
["ANAMET-M",8220293]
["ANAMET-M",8220296]
["ANAMET-M",8220299]
["ANAMET-M",8220300]
["ANAMET-M",8220303]
["ANAMET-M",8220306]
["ANAMET-M",8220309]
["ANAMET-M",8220310]
["ANAMET-M",8220313]
["ANAMET-M",8220316]
["ANAMET-M",8220319]
["ANAMET-M",8222090]
["ANAMET-M",8222093]
["ANAMET-M",8222096]
["ANAMET-M",8222099]
["ANAMET-M",8222100]
["ANAMET-M",8222103]
["ANAMET-M",8222106]
["ANAMET-M",8222109]
["ANAMET-M",8222110]
["ANAMET-M",8222113]
["ANAMET-M",8222116]
["ANAMET-M",8222119]
["ANAMET-M",8222120]
["ANAMET-M",8222123]
["ANAMET-M",8222126]
["ANAMET-M",8222129]
["ANAMET-M",8222130]
["ANAMET-M",8222133]
["ANAMET-M",8222136]
["ANAMET-M",8222139]
["ANAMET-M",8222140]
["ANAMET-M",8222143]
["ANAMET-M",8222146]
["ANAMET-M",8222149]
["ANAMET-M",8222150]
["ANAMET-M",8222153]
["ANAMET-M",8222156]
["ANAMET-M",8222159]
["ANAMET-M",8222180]
["ANAMET-M",8222183]
["ANAMET-M",8222186]
["ANAMET-M",8222189]
["ANAMET-M",8222190]
["ANAMET-M",8222193]
["ANAMET-M",8222196]
["ANAMET-M",8222199]
["ANAMET-M",8222230]
["ANAMET-M",8222233]
["ANAMET-M",8222236]
["ANAMET-M",8222239]
["ANAMET-M",8222240]
["ANAMET-M",8222243]
["ANAMET-M",8222246]
["ANAMET-M",8222249]
["ANAMET-M",8222250]
["ANAMET-M",8222253]
["ANAMET-M",8222256]
["ANAMET-M",8222259]
["ANAMET-M",8222290]
["ANAMET-M",8222293]
["ANAMET-M",8222296]
["ANAMET-M",8222299]
["ANAMET-M",8222300]
["ANAMET-M",8222303]
["ANAMET-M",8222306]
["ANAMET-M",8222309]
["ANAMET-M",8222310]
["ANAMET-M",8222313]
["ANAMET-M",8222316]
["ANAMET-M",8222319]
["ANAMET-M",8223090]
["ANAMET-M",8223093]
["ANAMET-M",8223096]
["ANAMET-M",8223099]
["ANAMET-M",8223100]
["ANAMET-M",8223103]
["ANAMET-M",8223106]
["ANAMET-M",8223109]
["ANAMET-M",8223110]
["ANAMET-M",8223113]
["ANAMET-M",8223116]
["ANAMET-M",8223119]
["ANAMET-M",8223120]
["ANAMET-M",8223123]
["ANAMET-M",8223126]
["ANAMET-M",8223129]
["ANAMET-M",8223130]
["ANAMET-M",8223133]
["ANAMET-M",8223136]
["ANAMET-M",8223139]
["ANAMET-M",8223140]
["ANAMET-M",8223143]
["ANAMET-M",8223146]
["ANAMET-M",8223149]
["ANAMET-M",8223150]
["ANAMET-M",8223153]
["ANAMET-M",8223156]
["ANAMET-M",8223159]
["ANAMET-M",8223180]
["ANAMET-M",8223183]
["ANAMET-M",8223186]
["ANAMET-M",8223189]
["ANAMET-M",8223190]
["ANAMET-M",8223193]
["ANAMET-M",8223196]
["ANAMET-M",8223199]
["ANAMET-M",8223230]
["ANAMET-M",8223233]
["ANAMET-M",8223236]
["ANAMET-M",8223239]
["ANAMET-M",8223240]
["ANAMET-M",8223243]
["ANAMET-M",8223246]
["ANAMET-M",8223249]
["ANAMET-M",8223250]
["ANAMET-M",8223253]
["ANAMET-M",8223256]
["ANAMET-M",8223259]
["ANAMET-M",8223290]
["ANAMET-M",8223293]
["ANAMET-M",8223296]
["ANAMET-M",8223299]
["ANAMET-M",8223300]
["ANAMET-M",8223303]
["ANAMET-M",8223306]
["ANAMET-M",8223309]
["ANAMET-M",8223310]
["ANAMET-M",8223313]
["ANAMET-M",8223316]
["ANAMET-M",8223319]
["ANAMET-M",8240100]
["ANAMET-M",8240103]
["ANAMET-M",8240106]
["ANAMET-M",8240109]
["ANAMET-M",8240110]
["ANAMET-M",8240113]
["ANAMET-M",8240116]
["ANAMET-M",8240119]
["ANAMET-M",8240120]
["ANAMET-M",8240123]
["ANAMET-M",8240126]
["ANAMET-M",8240129]
["ANAMET-M",8240130]
["ANAMET-M",8240133]
["ANAMET-M",8240136]
["ANAMET-M",8240139]
["ANAMET-M",8240140]
["ANAMET-M",8240143]
["ANAMET-M",8240146]
["ANAMET-M",8240149]
["ANAMET-M",8240150]
["ANAMET-M",8240153]
["ANAMET-M",8240156]
["ANAMET-M",8240159]
["ANAMET-M",8240180]
["ANAMET-M",8240183]
["ANAMET-M",8240186]
["ANAMET-M",8240189]
["ANAMET-M",8240190]
["ANAMET-M",8240193]
["ANAMET-M",8240196]
["ANAMET-M",8240199]
["ANAMET-M",8240230]
["ANAMET-M",8240233]
["ANAMET-M",8240236]
["ANAMET-M",8240239]
["ANAMET-M",8240240]
["ANAMET-M",8240243]
["ANAMET-M",8240246]
["ANAMET-M",8240249]
["ANAMET-M",8240250]
["ANAMET-M",8240253]
["ANAMET-M",8240256]
["ANAMET-M",8240259]
["ANAMET-M",8242100]
["ANAMET-M",8242103]
["ANAMET-M",8242106]
["ANAMET-M",8242109]
["ANAMET-M",8242110]
["ANAMET-M",8242113]
["ANAMET-M",8242116]
["ANAMET-M",8242119]
["ANAMET-M",8242120]
["ANAMET-M",8242123]
["ANAMET-M",8242126]
["ANAMET-M",8242129]
["ANAMET-M",8242130]
["ANAMET-M",8242133]
["ANAMET-M",8242136]
["ANAMET-M",8242139]
["ANAMET-M",8242140]
["ANAMET-M",8242143]
["ANAMET-M",8242146]
["ANAMET-M",8242149]
["ANAMET-M",8242150]
["ANAMET-M",8242153]
["ANAMET-M",8242156]
["ANAMET-M",8242159]
["ANAMET-M",8242180]
["ANAMET-M",8242183]
["ANAMET-M",8242186]
["ANAMET-M",8242189]
["ANAMET-M",8242190]
["ANAMET-M",8242193]
["ANAMET-M",8242196]
["ANAMET-M",8242199]
["ANAMET-M",8242230]
["ANAMET-M",8242233]
["ANAMET-M",8242236]
["ANAMET-M",8242239]
["ANAMET-M",8242240]
["ANAMET-M",8242243]
["ANAMET-M",8242246]
["ANAMET-M",8242249]
["ANAMET-M",8242250]
["ANAMET-M",8242253]
["ANAMET-M",8242256]
["ANAMET-M",8242259]
["ANAMET-M",8243090]
["ANAMET-M",8243093]
["ANAMET-M",8243096]
["ANAMET-M",8243099]
["ANAMET-M",8243100]
["ANAMET-M",8243103]
["ANAMET-M",8243106]
["ANAMET-M",8243109]
["ANAMET-M",8243110]
["ANAMET-M",8243113]
["ANAMET-M",8243116]
["ANAMET-M",8243119]
["ANAMET-M",8243120]
["ANAMET-M",8243123]
["ANAMET-M",8243126]
["ANAMET-M",8243129]
["ANAMET-M",8243130]
["ANAMET-M",8243133]
["ANAMET-M",8243136]
["ANAMET-M",8243139]
["ANAMET-M",8243140]
["ANAMET-M",8243143]
["ANAMET-M",8243146]
["ANAMET-M",8243149]
["ANAMET-M",8243150]
["ANAMET-M",8243153]
["ANAMET-M",8243156]
["ANAMET-M",8243159]
["ANAMET-M",8243180]
["ANAMET-M",8243183]
["ANAMET-M",8243186]
["ANAMET-M",8243189]
["ANAMET-M",8243190]
["ANAMET-M",8243193]
["ANAMET-M",8243196]
["ANAMET-M",8243199]
["ANAMET-M",8243230]
["ANAMET-M",8243233]
["ANAMET-M",8243236]
["ANAMET-M",8243239]
["ANAMET-M",8243240]
["ANAMET-M",8243243]
["ANAMET-M",8243246]
["ANAMET-M",8243249]
["ANAMET-M",8243250]
["ANAMET-M",8243253]
["ANAMET-M",8243256]
["ANAMET-M",8243259]
["ANAMET-M",8260160]
["ANAMET-M",8260169]
["ANAMET-M",8260200]
["ANAMET-M",8260209]
["ANAMET-M",8260250]
["ANAMET-M",8260259]
["ANAMET-M",8260320]
["ANAMET-M",8260329]
["ANAMET-M",8260400]
["ANAMET-M",8260409]
["ANAMET-M",8261160]
["ANAMET-M",8261169]
["ANAMET-M",8261200]
["ANAMET-M",8261209]
["ANAMET-M",8261250]
["ANAMET-M",8261259]
["ANAMET-M",8261320]
["ANAMET-M",8261329]
["ANAMET-M",8261400]
["ANAMET-M",8261409]
["ANAMET-M",8261500]
["ANAMET-M",8261509]
["ANAMET-M",8262160]
["ANAMET-M",8262169]
["ANAMET-M",8262200]
["ANAMET-M",8262209]
["ANAMET-M",8262250]
["ANAMET-M",8262259]
["ANAMET-M",8262320]
["ANAMET-M",8262329]
["ANAMET-M",8262400]
["ANAMET-M",8262409]
["ANAMET-M",8262500]
["ANAMET-M",8262509]
["ANAMET-M",8270120]
["ANAMET-M",8270129]
["ANAMET-M",8270160]
["ANAMET-M",8270169]
["ANAMET-M",8270200]
["ANAMET-M",8270209]
["ANAMET-M",8270260]
["ANAMET-M",8270269]
["ANAMET-M",8270350]
["ANAMET-M",8270359]
["ANAMET-M",8271120]
["ANAMET-M",8271129]
["ANAMET-M",8271160]
["ANAMET-M",8271169]
["ANAMET-M",8271200]
["ANAMET-M",8271209]
["ANAMET-M",8271260]
["ANAMET-M",8271269]
["ANAMET-M",8271350]
["ANAMET-M",8271359]
["ANAMET-M",8271400]
["ANAMET-M",8271409]
["ANAMET-M",8272160]
["ANAMET-M",8272169]
["ANAMET-M",8272200]
["ANAMET-M",8272209]
["ANAMET-M",8272260]
["ANAMET-M",8272269]
["ANAMET-M",8272350]
["ANAMET-M",8272359]
["ANAMET-M",8272400]
["ANAMET-M",8272409]
["ANAMET-M",8275110]
["ANAMET-M",8275119]
["ANAMET-M",8275130]
["ANAMET-M",8275139]
["ANAMET-M",8275160]
["ANAMET-M",8275169]
["ANAMET-M",8275210]
["ANAMET-M",8275219]
["ANAMET-M",8275290]
["ANAMET-M",8275299]
["ANAMET-M",8275360]
["ANAMET-M",8275369]
["ANAMET-M",8279991]
["ANAMET-M",8280169]
["ANAMET-M",8280209]
["ANAMET-M",8280259]
["ANAMET-M",8280329]
["ANAMET-M",8280409]
["ANAMET-S",8280509]
["ANAMET-S",8280609]
["ANAMET-S",8280639]
["ANAMET-M",8320169]
["ANAMET-M",8320209]
["ANAMET-M",8320259]
["ANAMET-M",8320329]
["ANAMET-S",8320409]
["ANAMET-S",8320509]
["ANAMET-S",8320639]
["ANAMET-M",8382209]
["ANAMET-M",8382269]
["ANAMET-M",8385209]
["ANAMET-M",8385269]
["ANAMET-M",8420160]
["ANAMET-M",8420170]
["ANAMET-M",8420200]
["ANAMET-M",8420250]
["ANAMET-M",8440120]
["ANAMET-M",8440160]
["ANAMET-M",8440180]
["ANAMET-M",8440200]
["ANAMET-M",8800070]
["ANAMET-M",8800090]
["ANAMET-M",8800110]
["ANAMET-M",8800119]
["ANAMET-M",8800130]
["ANAMET-M",8800139]
["ANAMET-M",8800160]
["ANAMET-M",8800169]
["ANAMET-M",8800210]
["ANAMET-M",8800219]
["ANAMET-M",8800290]
["ANAMET-M",8800299]
["ANAMET-M",8800360]
["ANAMET-M",8800369]
["ANAMET-M",8800420]
["ANAMET-M",8800480]
["ANAMET-M",8801120]
["ANAMET-M",8801160]
["ANAMET-M",8801168]
["ANAMET-M",8801169]
["ANAMET-M",8801200]
["ANAMET-M",8801208]
["ANAMET-M",8801209]
["ANAMET-M",8801250]
["ANAMET-M",8801258]
["ANAMET-M",8801259]
["ANAMET-M",8801320]
["ANAMET-M",8801328]
["ANAMET-M",8801329]
["ANAMET-M",8801400]
["ANAMET-M",8801408]
["ANAMET-M",8801409]
["ANAMET-M",8801500]
["ANAMET-M",8801630]
["ANAMET-M",8802160]
["ANAMET-M",8802168]
["ANAMET-M",8802169]
["ANAMET-M",8802200]
["ANAMET-M",8802208]
["ANAMET-M",8802209]
["ANAMET-M",8802260]
["ANAMET-M",8802268]
["ANAMET-M",8802269]
["ANAMET-M",8802350]
["ANAMET-M",8802358]
["ANAMET-M",8802359]
["ANAMET-M",8802400]
["ANAMET-M",8802408]
["ANAMET-M",8802500]
["ANAMET-M",8803160]
["ANAMET-M",8803169]
["ANAMET-M",8803200]
["ANAMET-M",8803209]
["ANAMET-M",8803260]
["ANAMET-M",8803269]
["ANAMET-M",8803350]
["ANAMET-M",8803359]
["ANAMET-M",8803400]
["ANAMET-M",8803409]
["ANAMET-M",8803500]
["ANAMET-M",8803509]
["ANAMET-M",8805100]
["ANAMET-M",8805110]
["ANAMET-M",8805120]
["ANAMET-M",8805130]
["ANAMET-M",8805160]
["ANAMET-M",8805200]
["ANAMET-M",8805210]
["ANAMET-M",8805250]
["ANAMET-M",8805270]
["ANAMET-M",8805290]
["ANAMET-M",8805320]
["ANAMET-M",8805350]
["ANAMET-M",8805360]
["ANAMET-M",8805420]
["ANAMET-M",8810070]
["ANAMET-M",8810080]
["ANAMET-M",8810090]
["ANAMET-M",8810110]
["ANAMET-M",8810120]
["ANAMET-M",8810130]
["ANAMET-M",8810150]
["ANAMET-M",8810160]
["ANAMET-M",8810210]
["ANAMET-M",8810290]
["ANAMET-M",8810360]
["ANAMET-M",8810420]
["ANAMET-M",8811070]
["ANAMET-M",8811090]
["ANAMET-M",8811110]
["ANAMET-M",8811160]
["ANAMET-M",8811210]
["ANAMET-M",8811290]
["ANAMET-M",8811360]
["ANAMET-S",8811480]
["ANAMET-M",8812160]
["ANAMET-M",8812200]
["ANAMET-M",8812250]
["ANAMET-M",8812320]
["ANAMET-M",8812400]
["ANAMET-M",8812500]
["ANAMET-M",8812630]
["ANAMET-M",8820090]
["ANAMET-M",8820110]
["ANAMET-M",8820120]
["ANAMET-M",8820130]
["ANAMET-M",8820160]
["ANAMET-M",8820170]
["ANAMET-M",8820180]
["ANAMET-M",8820210]
["ANAMET-M",8820290]
["ANAMET-M",8820360]
["ANAMET-M",8820420]
["ANAMET-M",8820480]
["ANAMET-M",8821110]
["ANAMET-M",8821160]
["ANAMET-M",8821210]
["ANAMET-M",8821290]
["ANAMET-M",8821360]
["ANAMET-M",8821480]
["ANAMET-M",8822120]
["ANAMET-M",8822160]
["ANAMET-M",8822200]
["ANAMET-M",8822250]
["ANAMET-M",8822320]
["ANAMET-M",8822400]
["ANAMET-M",8822500]
["ANAMET-M",8823090]
["ANAMET-M",8823110]
["ANAMET-M",8823130]
["ANAMET-M",8823160]
["ANAMET-M",8823210]
["ANAMET-M",8823260]
["ANAMET-M",8823290]
["ANAMET-M",8823300]
["ANAMET-M",8823360]
["ANAMET-M",8823400]
["ANAMET-M",8823420]
["ANAMET-M",8823480]
["ANAMET-M",8824100]
["ANAMET-M",8824110]
["ANAMET-M",8824120]
["ANAMET-M",8824130]
["ANAMET-M",8824160]
["ANAMET-M",8824200]
["ANAMET-M",8824350]
["ANAMET-M",8824400]
["ANAMET-M",8824500]
["ANAMET-M",8825160]
["ANAMET-M",8825200]
["ANAMET-M",8825220]
["ANAMET-M",8825240]
["ANAMET-M",8825250]
["ANAMET-M",8825270]
["ANAMET-M",8825280]
["ANAMET-M",8825320]
["ANAMET-M",8825360]
["ANAMET-M",8825380]
["ANAMET-M",8825400]
["ANAMET-S",8825480]
["ANAMET-S",8825500]
["ANAMET-S",8825520]
["ANAMET-S",8825600]
["ANAMET-S",8825630]
["ANAMET-M",8826120]
["ANAMET-M",8826160]
["ANAMET-M",8826200]
["ANAMET-M",8826260]
["ANAMET-M",8832080]
["ANAMET-M",8832120]
["ANAMET-M",8832180]
["ANAMET-M",8832300]
["ANAMET-M",8833080]
["ANAMET-M",8833086]
["ANAMET-M",8833087]
["ANAMET-M",8833100]
["ANAMET-M",8833106]
["ANAMET-M",8833107]
["ANAMET-M",8833120]
["ANAMET-M",8833126]
["ANAMET-M",8833127]
["ANAMET-M",8833140]
["ANAMET-M",8833146]
["ANAMET-M",8833147]
["ANAMET-M",8833160]
["ANAMET-M",8833166]
["ANAMET-M",8833167]
["ANAMET-M",8833180]
["ANAMET-M",8833186]
["ANAMET-M",8833187]
["ANAMET-M",8833200]
["ANAMET-M",8833340]
["ANAMET-M",8834160]
["ANAMET-M",8834200]
["ANAMET-M",8834260]
["ANAMET-M",8834350]
["ANAMET-M",8834400]
["ANAMET-S",8834500]
["ANAMET-M",8840080]
["ANAMET-M",8840120]
["ANAMET-M",8840140]
["ANAMET-M",8840180]
["ANAMET-M",8840300]
["ANAMET-M",8850160]
["ANAMET-M",8850162]
["ANAMET-M",8850200]
["ANAMET-M",8850202]
["ANAMET-M",8850260]
["ANAMET-M",8850262]
["ANAMET-M",8850350]
["ANAMET-M",8850352]
["ANAMET-M",8850402]
["ANAMET-M",8850502]
["ANAMET-M",8852160]
["ANAMET-M",8852161]
["ANAMET-M",8852200]
["ANAMET-M",8852201]
["ANAMET-M",8852250]
["ANAMET-M",8852251]
["ANAMET-M",8852320]
["ANAMET-M",8852321]
["ANAMET-M",8852400]
["ANAMET-M",8852401]
["ANAMET-M",8853060]
["ANAMET-M",8853100]
["ANAMET-M",8853120]
["ANAMET-M",8853160]
["ANAMET-M",8853200]
["ANAMET-M",8853260]
["ANAMET-M",8853350]
["ANAMET-M",8853400]
["ANAMET-M",8853500]
["ANAMET-S",8853630]
["ANAMET-M",71411292]
["ANAMET-M",71411692]
["ANAMET-M",71412092]
["ANAMET-M",71412692]
["ANAMET-M",71413592]
["ANAMET-M",71414092]
["ANAMET-M",71415092]
["ANAMET-M",71451292]
["ANAMET-M",71451692]
["ANAMET-M",71452092]
["ANAMET-M",71452692]
["ANAMET-M",71453592]
["ANAMET-M",71454092]
["ANAMET-M",71455092]
["TECHNIK","  156 SV-V"]
["TECHNIK","  250 SV-T-V-K"]
["TECHNIK","  416 SV-V"]
["TECHNIK","  625 SV-S-V"]
["TECHNIK","  625 SV-T-V-K"]
["TECHNIK","  625 SV-V"]
["TECHNIK"," 1695 SV-T-V-K"]
["TECHNIK"," 35185 SV-T-V-K"]
["TECHNIK"," 50240 SV-T-V-K"]
["TECHNIK SPECIAL - AKCIA","02056 kufr"]
["TECHNIK SPECIAL - AKCIA","02059 kufr"]
["TECHNIK SPECIAL - AKCIA","02062 kufr"]
["TECHNIK SPECIAL - AKCIA","10 ALU-22"]
["TECHNIK SPECIAL - AKCIA","10 ALU-45"]
["TECHNIK SPECIAL - AKCIA","10 ALU-50"]
["TECHNIK SPECIAL - AKCIA","10 C"]
["TECHNIK SPECIAL - AKCIA","10 CU-22"]
["TECHNIK SPECIAL - AKCIA","10 CU-3D"]
["TECHNIK SPECIAL - AKCIA","10 CU-45"]
["TECHNIK SPECIAL - AKCIA","10 CU-50"]
["TECHNIK SPECIAL - AKCIA","12 ALU-22"]
["TECHNIK SPECIAL - AKCIA","12 ALU-45"]
["TECHNIK SPECIAL - AKCIA","12 ALU-50"]
["TECHNIK SPECIAL - AKCIA","12 C"]
["TECHNIK SPECIAL - AKCIA","12 CU-22"]
["TECHNIK SPECIAL - AKCIA","12 CU-3D"]
["TECHNIK SPECIAL - AKCIA","12 CU-45"]
["TECHNIK SPECIAL - AKCIA","12 CU-50"]
["TECHNIK SPECIAL - AKCIA","14 ALU-22"]
["TECHNIK SPECIAL - AKCIA","14 ALU-45"]
["TECHNIK SPECIAL - AKCIA","14 ALU-50"]
["TECHNIK SPECIAL - AKCIA","14 C"]
["TECHNIK SPECIAL - AKCIA","14 CU-22"]
["TECHNIK SPECIAL - AKCIA","14 CU-3D"]
["TECHNIK SPECIAL - AKCIA","14 CU-45"]
["TECHNIK SPECIAL - AKCIA","14 CU-50"]
["TECHNIK","150240 SV-T-K"]
["TECHNIK","150240 SV-T-V-K"]
["TECHNIK SPECIAL - AKCIA","16 ALU-22"]
["TECHNIK SPECIAL - AKCIA","16 ALU-45"]
["TECHNIK SPECIAL - AKCIA","16 ALU-50"]
["TECHNIK SPECIAL - AKCIA","16 C"]
["TECHNIK SPECIAL - AKCIA","16 CU-22"]
["TECHNIK SPECIAL - AKCIA","16 CU-3D"]
["TECHNIK SPECIAL - AKCIA","16 CU-45"]
["TECHNIK SPECIAL - AKCIA","16 CU-50"]
["TECHNIK SPECIAL - AKCIA","18 ALU-22"]
["TECHNIK SPECIAL - AKCIA","18 ALU-45"]
["TECHNIK SPECIAL - AKCIA","18 ALU-450"]
["TECHNIK SPECIAL - AKCIA","18 ALU-50"]
["TECHNIK SPECIAL - AKCIA","18 ALU-60"]
["TECHNIK SPECIAL - AKCIA","18 C"]
["TECHNIK SPECIAL - AKCIA","18 CU-22"]
["TECHNIK SPECIAL - AKCIA","18 CU-3D"]
["TECHNIK SPECIAL - AKCIA","18 CU-45"]
["TECHNIK SPECIAL - AKCIA","18 CU-50"]
["TECHNIK SPECIAL - AKCIA","20 C"]
["TECHNIK SPECIAL - AKCIA","20 CU-22"]
["TECHNIK SPECIAL - AKCIA","20 CU-3D"]
["TECHNIK SPECIAL - AKCIA","20 CU-45"]
["TECHNIK SPECIAL - AKCIA","20 CU-50"]
["TECHNIK SPECIAL - AKCIA","21 ALU-22"]
["TECHNIK SPECIAL - AKCIA","22 ALU-22"]
["TECHNIK SPECIAL - AKCIA","22 ALU-45"]
["TECHNIK SPECIAL - AKCIA","22 ALU-450"]
["TECHNIK SPECIAL - AKCIA","22 ALU-50"]
["TECHNIK SPECIAL - AKCIA","22 C"]
["TECHNIK SPECIAL - AKCIA","22 CU-22"]
["TECHNIK SPECIAL - AKCIA","22 CU-3D"]
["TECHNIK SPECIAL - AKCIA","22 CU-45"]
["TECHNIK SPECIAL - AKCIA","22 CU-50"]
["TECHNIK SPECIAL - AKCIA","25 ALU-22"]
["TECHNIK SPECIAL - AKCIA","25 ALU-50"]
["TECHNIK SPECIAL - AKCIA","25 C"]
["TECHNIK SPECIAL - AKCIA","25 CU-22"]
["TECHNIK SPECIAL - AKCIA","25 CU-3D"]
["TECHNIK SPECIAL - AKCIA","25 CU-50"]
["TECHNIK SPECIAL - AKCIA","25 CU-60"]
["TECHNIK SPECIAL - AKCIA","28 ALU-19"]
["TECHNIK SPECIAL - AKCIA","28 ALU-22"]
["TECHNIK SPECIAL - AKCIA","28 ALU-50"]
["TECHNIK SPECIAL - AKCIA","28 C"]
["TECHNIK SPECIAL - AKCIA","28 C-ALU"]
["TECHNIK SPECIAL - AKCIA","28 CU-19"]
["TECHNIK SPECIAL - AKCIA","28 CU-22"]
["TECHNIK SPECIAL - AKCIA","28 CU-3D"]
["TECHNIK SPECIAL - AKCIA","28 CU-450"]
["TECHNIK SPECIAL - AKCIA","28 CU-50"]
["TECHNIK SPECIAL - AKCIA","32 ALU-22"]
["TECHNIK SPECIAL - AKCIA","32 ALU-450"]
["TECHNIK SPECIAL - AKCIA","32 ALU-50"]
["TECHNIK SPECIAL - AKCIA","32 C"]
["TECHNIK SPECIAL - AKCIA","32 C-ALU"]
["TECHNIK SPECIAL - AKCIA","32 CU-3D"]
["TECHNIK SPECIAL - AKCIA","32 CU-450"]
["TECHNIK SPECIAL - AKCIA","34 ALU-22"]
["TECHNIK SPECIAL - AKCIA","34 ALU-450"]
["TECHNIK SPECIAL - AKCIA","34 C-ALU"]
["TECHNIK SPECIAL - AKCIA","34 CU-3D"]
["TECHNIK SPECIAL - AKCIA","34 CU-520"]
["TECHNIK SPECIAL - AKCIA","38 CU-1000"]
["TECHNIK SPECIAL - AKCIA","38 CU-3D"]
["TECHNIK SPECIAL - AKCIA","38 CU-450"]
["TECHNIK SPECIAL - AKCIA","38 CU-520"]
["TECHNIK","3HTI  1,5 černá"]
["TECHNIK","3HTI  1,5 černá R"]
["TECHNIK","3HTI  1,5 žlutá R"]
["TECHNIK","3HTI  1,5 žz"]
["TECHNIK","3HTI  1,5 žz R"]
["TECHNIK","3HTI  3,0 bílá"]
["TECHNIK","3HTI  3,0 bílá T2"]
["TECHNIK","3HTI  3,0 černá"]
["TECHNIK","3HTI  3,0 černá R"]
["TECHNIK","3HTI  3,0 žlutá"]
["TECHNIK","3HTI  3,0 žlutá T2"]
["TECHNIK","3HTI  3,0 žz R"]
["TECHNIK","3HTI  4,5 bílá T1"]
["TECHNIK","3HTI  4,5 černá"]
["TECHNIK","3HTI  4,5 černá R"]
["TECHNIK","3HTI  4,5 transp R"]
["TECHNIK","3HTI  4,5 žlutá R"]
["TECHNIK","3HTI  4,5 žlutá T1"]
["TECHNIK","3HTI  4,5 žz R"]
["TECHNIK","3HTI  6,0 bílá"]
["TECHNIK","3HTI  6,0 bílá T1"]
["TECHNIK","3HTI  6,0 černá"]
["TECHNIK","3HTI  6,0 černá R"]
["TECHNIK","3HTI  6,0 žlutá"]
["TECHNIK","3HTI  6,0 žlutá T1"]
["TECHNIK","3HTI  6,0 žz R"]
["TECHNIK","3HTI  9,0 černá"]
["TECHNIK","3HTI  9,0 černá R"]
["TECHNIK","3HTI  9,0 modrá R"]
["TECHNIK","3HTI  9,0 rudá R"]
["TECHNIK","3HTI  9,0 žz R"]
["TECHNIK","3HTI 12,0 černá"]
["TECHNIK","3HTI 12,0 černá R"]
["TECHNIK","3HTI 12,0 modrá R"]
["TECHNIK","3HTI 12,0 žz R"]
["TECHNIK","3HTI 18,0 bílá R"]
["TECHNIK","3HTI 18,0 černá"]
["TECHNIK","3HTI 18,0 černá R"]
["TECHNIK","3HTI 18,0 černá R."]
["TECHNIK","3HTI 18,0 rudá R"]
["TECHNIK","3HTI 18,0 transp R"]
["TECHNIK","3HTI 18,0 žz R"]
["TECHNIK","3HTI 24,0 bílá R"]
["TECHNIK","3HTI 24,0 černá"]
["TECHNIK","3HTI 24,0 černá R"]
["TECHNIK","3HTI 24,0 zelená R"]
["TECHNIK","3HTI 24,0 žz R"]
["TECHNIK","3HTI 39,0 černá"]
["TECHNIK","3HTI 39,0 černá R"]
["TECHNIK","3HTI 39,0 modrá R"]
["TECHNIK","3HTI 39,0 rudá R"]
["TECHNIK","3HTI 39,0 žz R"]
["TECHNIK SPECIAL - AKCIA","42 ALU-450"]
["TECHNIK SPECIAL - AKCIA","42 CU-3D"]
["TECHNIK SPECIAL - AKCIA","42 CU-450"]
["TECHNIK SPECIAL - AKCIA","42 CU-520"]
["TECHNIK SPECIAL - AKCIA","44 ALU-450"]
["TECHNIK SPECIAL - AKCIA","44 CU-1000"]
["TECHNIK SPECIAL - AKCIA","44 CU-3D"]
["TECHNIK SPECIAL - AKCIA","44 CU-450"]
["TECHNIK SPECIAL - AKCIA","44 CU-520"]
["TECHNIK","451"]
["TECHNIK","45-120"]
["TECHNIK","45-120-341"]
["TECHNIK","45-121"]
["TECHNIK","45-125"]
["TECHNIK","45-125-341"]
["TECHNIK","452"]
["TECHNIK","454"]
["TECHNIK SPECIAL - AKCIA","48 CU-520"]
["TECHNIK SPECIAL - AKCIA","5 CU-22"]
["TECHNIK SPECIAL - AKCIA","5 CU-45"]
["TECHNIK SPECIAL - AKCIA","5 CU-50"]
["TECHNIK SPECIAL - AKCIA","52 ALU-450"]
["TECHNIK SPECIAL - AKCIA","52 CU-450"]
["TECHNIK SPECIAL - AKCIA","52 CU-520"]
["TECHNIK SPECIAL - AKCIA","58 ALU-450"]
["TECHNIK SPECIAL - AKCIA","58 CU-450"]
["TECHNIK SPECIAL - AKCIA","58 CU-520"]
["TECHNIK SPECIAL - AKCIA","6 C"]
["TECHNIK SPECIAL - AKCIA","6 CU-22"]
["TECHNIK SPECIAL - AKCIA","6 CU-45"]
["TECHNIK SPECIAL - AKCIA","6 CU-50"]
["TECHNIK SPECIAL - AKCIA","60 ALU-450"]
["TECHNIK SPECIAL - AKCIA","60 CU-1000"]
["TECHNIK SPECIAL - AKCIA","60 CU-520"]
["TECHNIK","71 B"]
["ANAMET-M","7120169-6"]
["ANAMET-M","7120179-6"]
["ANAMET-M","7120209-6"]
["ANAMET-M","7120259-6"]
["ANAMET-M","7120329-6"]
["ANAMET-M","7120409-6"]
["ANAMET-M","7129169-6"]
["ANAMET-M","7129179-6"]
["ANAMET-M","7129209-6"]
["ANAMET-M","7129259-6"]
["ANAMET-M","7129329-6"]
["ANAMET-M","7129409-6"]
["ANAMET-M","7140129-2"]
["ANAMET-M","7140129-6"]
["ANAMET-M","7140169-2"]
["ANAMET-M","7140169-6"]
["ANAMET-M","7140209-2"]
["ANAMET-M","7140209-6"]
["ANAMET-M","7140269-2"]
["ANAMET-M","7140269-6"]
["ANAMET-M","7140359-2"]
["ANAMET-M","7140359-6"]
["ANAMET-M","7140409-2"]
["ANAMET-M","7140509-2"]
["ANAMET-M","7149129-2"]
["ANAMET-S","7149129-2"]
["ANAMET-M","7149129-6"]
["ANAMET-S","7149129-6"]
["ANAMET-M","7149169-2"]
["ANAMET-S","7149169-2"]
["ANAMET-M","7149169-6"]
["ANAMET-S","7149169-6"]
["ANAMET-M","7149-209-2"]
["ANAMET-S","7149-209-2"]
["ANAMET-M","7149209-6"]
["ANAMET-S","7149209-6"]
["ANAMET-M","7149-269-2"]
["ANAMET-S","7149-269-2"]
["ANAMET-M","7149269-6"]
["ANAMET-S","7149269-6"]
["ANAMET-M","7149359-2"]
["ANAMET-S","7149359-2"]
["ANAMET-M","7149359-6"]
["ANAMET-S","7149359-6"]
["ANAMET-M","7149409-2"]
["ANAMET-S","7149409-2"]
["ANAMET-M","7149509-2"]
["ANAMET-S","7149509-2"]
["TECHNIK","72 B"]
["TECHNIK","73 B"]
["TECHNIK","74 B"]
["TECHNIK","76 B"]
["TECHNIK SPECIAL - AKCIA","8 C"]
["TECHNIK SPECIAL - AKCIA","8 CU-22"]
["TECHNIK SPECIAL - AKCIA","8 CU-3D"]
["TECHNIK SPECIAL - AKCIA","8 CU-45"]
["TECHNIK SPECIAL - AKCIA","8 CU-50"]
["ANAMET-M","8107117-3"]
["ANAMET-S","8107117-3"]
["ANAMET-M","8107157-3"]
["ANAMET-S","8107157-3"]
["ANAMET-M","8107167-3"]
["ANAMET-S","8107167-3"]
["ANAMET-M","8107217-3"]
["ANAMET-S","8107217-3"]
["ANAMET-M","8127157-3"]
["ANAMET-S","8127157-3"]
["ANAMET-M","8127167-3"]
["ANAMET-S","8127167-3"]
["ANAMET-M","8127207-3"]
["ANAMET-S","8127207-3"]
["ANAMET-M","8127227-3"]
["ANAMET-S","8127227-3"]
["TECHNIK","92-BLK-PR443U"]
["TECHNIK","94-7872-C425"]
["TECHNIK","98-WT31-1242"]
["TECHNIK SPECIAL - AKCIA","A3-MO 01475/28"]
["TECHNIK SPECIAL - AKCIA","A3-MO 056/68"]
["TECHNIK SPECIAL - AKCIA","A3-OI 056/68"]
["TECHNIK SPECIAL - AKCIA","A4-MO 2,8"]
["TECHNIK SPECIAL - AKCIA","A4-MO 4,8"]
["TECHNIK SPECIAL - AKCIA","A4-MO 6,3"]
["TECHNIK SPECIAL - AKCIA","AB 01"]
["TECHNIK SPECIAL - AKCIA","AC 25"]
["TECHNIK SPECIAL - AKCIA","AC 25 T"]
["TECHNIK SPECIAL - AKCIA","AC 40"]
["TECHNIK SPECIAL - AKCIA","AC 40 T"]
["TECHNIK SPECIAL - AKCIA","AC100"]
["TECHNIK SPECIAL - AKCIA","AC100 T"]
["TECHNIK SPECIAL - AKCIA","AC-DX"]
["TECHNIK","AD-24ESEU"]
["TECHNIK","AD-E001"]
["REIKU-B","AFFSS-M10"]
["REIKU-B","AFFSS-M12"]
["REIKU-B","AFFSS-M16"]
["REIKU-B","AFFSS-M20"]
["REIKU-B","AFFSS-M25"]
["REIKU-B","AFFSS-M32"]
["REIKU-B","AFFSS-M40"]
["REIKU-B","AFFSS-M50"]
["REIKU-B","AFFSS-M63"]
["REIKU-B","AFFSS-P07"]
["REIKU-B","AFFSS-P09"]
["REIKU-B","AFFSS-P11"]
["REIKU-B","AFFSS-P13"]
["REIKU-B","AFFSS-P16"]
["REIKU-B","AFFSS-P21"]
["REIKU-B","AFFSS-P29"]
["REIKU-B","AFFSS-P36"]
["REIKU-B","AFFSS-P42"]
["REIKU-B","AFFSS-P48"]
["TECHNIK SPECIAL - AKCIA","AHP 03"]
["TECHNIK SPECIAL - AKCIA","AI 01"]
["TECHNIK SPECIAL - AKCIA","AI 02"]
["TECHNIK SPECIAL - AKCIA","AI 03"]
["TECHNIK SPECIAL - AKCIA","AI 04"]
["TECHNIK SPECIAL - AKCIA","AKKU 18,0 V"]
["TECHNIK SPECIAL - AKCIA","AKKU COMPACT"]
["TECHNIK SPECIAL - AKCIA","AKKU COMPACT SET"]
["TECHNIK","AKR 1 - 60/24"]
["TECHNIK","AKR 2 - 75/30"]
["TECHNIK","AKR 3 - 110/45"]
["TECHNIK","AKR 4 - 135/55"]
["TECHNIK","AKR 5 - 175/55"]
["TECHNIK","AL 10"]
["TECHNIK","AL 16"]
["TECHNIK","AL 16-M 8"]
["TECHNIK","AL 16-M10"]
["TECHNIK","AL 25"]
["TECHNIK","AL 25-M 8"]
["TECHNIK","AL 25-M10"]
["TECHNIK","AL 25-M12"]
["TECHNIK","AL 35"]
["TECHNIK","AL 35-M 8"]
["TECHNIK","AL 35-M10"]
["TECHNIK","AL 35-M12"]
["TECHNIK","AL 50"]
["TECHNIK","AL 50-M 8"]
["TECHNIK","AL 50-M10"]
["TECHNIK","AL 50-M12"]
["TECHNIK","AL 70"]
["TECHNIK","AL 70-M 8"]
["TECHNIK","AL 70-M10"]
["TECHNIK","AL 70-M12"]
["TECHNIK","AL 95"]
["TECHNIK","AL 95-M10"]
["TECHNIK","AL 95-M12"]
["TECHNIK","AL120"]
["TECHNIK","AL120-M10"]
["TECHNIK","AL120-M12"]
["TECHNIK","AL120-M16"]
["TECHNIK","AL150"]
["TECHNIK","AL150-M10"]
["TECHNIK","AL150-M12"]
["TECHNIK","AL150-M16"]
["TECHNIK","AL185"]
["TECHNIK","AL185-M10"]
["TECHNIK","AL185-M12"]
["TECHNIK","AL185-M16"]
["TECHNIK","AL240"]
["TECHNIK","AL240-M10"]
["TECHNIK","AL240-M12"]
["TECHNIK","AL240-M16"]
["TECHNIK","AL300"]
["TECHNIK","AL300-M12"]
["TECHNIK","AL300-M16"]
["TECHNIK","AL400-M12"]
["TECHNIK","AL400-M16"]
["TECHNIK","AL500"]
["TECHNIK","AL500-M12"]
["TECHNIK","AL500-M16"]
["TECHNIK","AL625-M16"]
["TECHNIK SPECIAL - AKCIA","ALC/5,5"]
["TECHNIK SPECIAL - AKCIA","ALC/6"]
["TECHNIK SPECIAL - AKCIA","ALC/7"]
["TECHNIK SPECIAL - AKCIA","ALC/PO 12x6,4"]
["TECHNIK SPECIAL - AKCIA","ALC/PR 12x6,4"]
["TECHNIK SPECIAL - AKCIA","ALC-02"]
["TECHNIK SPECIAL - AKCIA","ALC-H"]
["TECHNIK SPECIAL - AKCIA","ALC-R1 AKCE"]
["TECHNIK SPECIAL - AKCIA","ALC-R2"]
["TECHNIK","AL-F  16-M 8"]
["TECHNIK","AL-F  16-M10"]
["TECHNIK","AL-F  25-M 8"]
["TECHNIK","AL-F  25-M10"]
["TECHNIK","AL-F  25-M12"]
["TECHNIK","AL-F  35-M 8"]
["TECHNIK","AL-F  35-M10"]
["TECHNIK","AL-F  35-M12"]
["TECHNIK","AL-F  50-M 8"]
["TECHNIK","AL-F  50-M10"]
["TECHNIK","AL-F  50-M12"]
["TECHNIK","AL-F  70-M 8"]
["TECHNIK","AL-F  70-M10"]
["TECHNIK","AL-F  70-M12"]
["TECHNIK","AL-F  70-M16"]
["TECHNIK","AL-F  95-M10"]
["TECHNIK","AL-F  95-M12"]
["TECHNIK","AL-F  95-M16"]
["TECHNIK","AL-F 120-M10"]
["TECHNIK","AL-F 120-M12"]
["TECHNIK","AL-F 120-M16"]
["TECHNIK","AL-F 150-M10"]
["TECHNIK","AL-F 150-M12"]
["TECHNIK","AL-F 150-M16"]
["TECHNIK","AL-F 185-M10"]
["TECHNIK","AL-F 185-M12"]
["TECHNIK","AL-F 185-M16"]
["TECHNIK","AL-F 240-M10"]
["TECHNIK","AL-F 240-M12"]
["TECHNIK","AL-F 240-M16"]
["TECHNIK","AL-F 300-M12"]
["TECHNIK","AL-F 300-M16"]
["TECHNIK","AL-F 400-M12"]
["TECHNIK","AL-F 400-M16"]
["TECHNIK","AL-F 500-M12"]
["TECHNIK","AL-F 500-M16"]
["TECHNIK","AL-F 625-M16"]
["TECHNIK SPECIAL - AKCIA","ALFRA 03910"]
["TECHNIK","ALFRA 1101124"]
["TECHNIK","AL-ZE 10"]
["TECHNIK","AL-ZE 16"]
["TECHNIK","AL-ZE 25"]
["TECHNIK","AL-ZE 35"]
["TECHNIK","AL-ZE 50"]
["TECHNIK","AL-ZE 70"]
["TECHNIK","AL-ZE 95"]
["TECHNIK","AL-ZE120"]
["TECHNIK","AL-ZE150"]
["TECHNIK","AL-ZE185"]
["TECHNIK","AL-ZE240"]
["TECHNIK","AL-ZE300"]
["TECHNIK","AL-ZE500"]
["TECHNIK","AM  1"]
["TECHNIK","AM  5-28"]
["TECHNIK","AM  8-25"]
["TECHNIK SPECIAL - AKCIA","AM 02"]
["TECHNIK SPECIAL - AKCIA","AM 02 C"]
["TECHNIK SPECIAL - AKCIA","AM 02.1"]
["TECHNIK SPECIAL - AKCIA","AM 02-0,5/2,5"]
["TECHNIK SPECIAL - AKCIA","AM 04"]
["TECHNIK","AM 15-36"]
["TECHNIK","AM 20-60"]
["TECHNIK","AM 25 H"]
["TECHNIK","AM 25 P"]
["TECHNIK","AM 35 H"]
["TECHNIK","AM 35 P"]
["TECHNIK","AM-K"]
["TECHNIK","AM-M"]
["TECHNIK","AM-MI"]
["TECHNIK","AM-R"]
["TECHNIK","AM-X"]
["TECHNIK SPECIAL - AKCIA","ANP 8 STD"]
["TECHNIK SPECIAL - AKCIA","AP  35/2"]
["TECHNIK SPECIAL - AKCIA","AP  62"]
["TECHNIK SPECIAL - AKCIA","AP  62 D"]
["TECHNIK SPECIAL - AKCIA","AP 130"]
["TECHNIK SPECIAL - AKCIA","AP 132 C26"]
["TECHNIK SPECIAL - AKCIA","AP 132 C32"]
["TECHNIK SPECIAL - AKCIA","AP 132 C38"]
["TECHNIK SPECIAL - AKCIA","AP 132 U"]
["TECHNIK SPECIAL - AKCIA","AS 32"]
["TECHNIK SPECIAL - AKCIA","AS 34"]
["TECHNIK SPECIAL - AKCIA","AS 52"]
["TECHNIK SPECIAL - AKCIA","ASN 15"]
["TECHNIK SPECIAL - AKCIA","ASN 15 R"]
["TECHNIK SPECIAL - AKCIA","ASN 20"]
["TECHNIK SPECIAL - AKCIA","ASN 20 R"]
["TECHNIK","AT-44"]
["TECHNIK SPECIAL - AKCIA","AU 230-130 D"]
["TECHNIK SPECIAL - AKCIA","AU 450-130 D"]
["TECHNIK SPECIAL - AKCIA","AU 520-130 C"]
["TECHNIK SPECIAL - AKCIA","B 131-C"]
["TECHNIK SPECIAL - AKCIA","B 131LN-C"]
["TECHNIK SPECIAL - AKCIA","B 131-UC"]
["TECHNIK SPECIAL - AKCIA","B 1350-C"]
["TECHNIK SPECIAL - AKCIA","B 1350L-C"]
["TECHNIK SPECIAL - AKCIA","B 1350-UC"]
["TECHNIK SPECIAL - AKCIA","B 15 D"]
["TECHNIK SPECIAL - AKCIA","B 200"]
["TECHNIK SPECIAL - AKCIA","B 35-45 D"]
["TECHNIK SPECIAL - AKCIA","B 35-50 D"]
["TECHNIK SPECIAL - AKCIA","B 46"]
["TECHNIK SPECIAL - AKCIA","B 500"]
["TECHNIK SPECIAL - AKCIA","B 62"]
["TECHNIK SPECIAL - AKCIA","B70M-P24"]
["TECHNIK","BA-7000"]
["TECHNIK","BA-E001"]
["REIKU-B","Basic piece for sizes NW23 till NW29, reduceable to NW07"]
["BIMED","BBOS-11"]
["BIMED","BBOS-12"]
["BIMED","BBS-11"]
["BIMED","BBS-12"]
["BIMED","BBS-13"]
["BIMED","BBS-14"]
["BIMED","BBS-15"]
["BIMED","BBS-16"]
["BIMED","BBS-17"]
["BIMED","BBS-18"]
["BIMED","BBS-21"]
["BIMED","BBS-22"]
["BIMED","BBS-23"]
["BIMED","BBS-24"]
["BIMED","BBS-25"]
["BIMED","BBS-26"]
["BIMED","BBS-27"]
["BIMED","BBS-28"]
["BIMED","BBVP-01"]
["BIMED","BBVP-0S"]
["TECHNIK SPECIAL - AKCIA","BC 25"]
["TECHNIK SPECIAL - AKCIA","BC 55"]
["TECHNIK SPECIAL - AKCIA","BC 85"]
["TECHNIK SPECIAL - AKCIA","BC 90"]
["BIMED","BD-11"]
["BIMED","BD-12"]
["BIMED","BD-13"]
["BIMED","BD-14"]
["BIMED","BD-15"]
["BIMED","BD-16"]
["BIMED","BD-17"]
["BIMED","BD-18"]
["BIMED","BDSM-08"]
["BIMED","BDSM-09"]
["BIMED","BDSM-09S"]
["BIMED","BDSM-10"]
["BIMED","BDSM-10R"]
["BIMED","BDSM-11"]
["BIMED","BDSM-11R"]
["BIMED","BDSM-12"]
["TECHNIK","BENNING kabely 2"]
["TECHNIK","BENNING kabely 4"]
["TECHNIK","BENNING pouzdro I"]
["TECHNIK","BENNING pouzdro II"]
["BIMED","BEX-16/20"]
["TECHNIK","BF 190P"]
["TECHNIK","BF 55"]
["TECHNIK SPECIAL - AKCIA","B-FC 48N"]
["TECHNIK SPECIAL - AKCIA","B-FL 750"]
["TECHNIK","Bio - Cut"]
["TECHNIK","Bio - Fluid"]
["REIKU-B","BIORRB-12F"]
["REIKU-B","BIORRB-17F"]
["REIKU-B","BIORRB-23F"]
["REIKU-B","BIORRB-29F"]
["REIKU-B","BIORRB-36G"]
["REIKU-B","BIORRB-48G"]
["REIKU-B","BIORRB-52G"]
["REIKU-B","BIORRB-70G"]
["BIMED","BL-01"]
["BIMED","BL-02"]
["BIMED","BL-03"]
["BIMED","BL-04"]
["BIMED","BL-05"]
["BIMED","BL-06"]
["BIMED","BL-07"]
["BIMED","BL-08"]
["BIMED","BL-09"]
["BIMED","BL-10"]
["BIMED","BL-11"]
["BIMED","BL-12"]
["BIMED","BL-13"]
["BIMED","BL-14"]
["BIMED","BL-15"]
["BIMED","BL-16"]
["BIMED","BL-17"]
["BIMED","BL-18"]
["BIMED","BL-19"]
["BIMED","BL-20"]
["BIMED","BL-21"]
["BIMED","BL-22"]
["BIMED","BL-23"]
["BIMED","BL-24"]
["BIMED","BL-25"]
["BIMED","BL-26"]
["BIMED","BL-27"]
["BIMED","BL-28"]
["BIMED","BL-29"]
["BIMED","BL-30"]
["TECHNIK","BLACK SEAL SILIKON"]
["BIMED","BM-01"]
["BIMED","BM-01L"]
["BIMED","BM-02"]
["BIMED","BM-02L"]
["BIMED","BM-03"]
["BIMED","BM-04"]
["BIMED","BM-05"]
["BIMED","BM-06"]
["BIMED","BM-07"]
["BIMED","BM-08"]
["BIMED","BM-09"]
["BIMED","BM-0S"]
["BIMED","BM-10"]
["BIMED","BM-11"]
["BIMED","BM-11L"]
["BIMED","BM-12"]
["BIMED","BM-12L"]
["BIMED","BM-13"]
["BIMED","BM-14"]
["BIMED","BM-15"]
["BIMED","BM-16"]
["BIMED","BM-17"]
["BIMED","BM-18"]
["BIMED","BM-19"]
["BIMED","BM-1S"]
["BIMED","BM-20"]
["BIMED","BM-21"]
["BIMED","BM-21L"]
["BIMED","BM-22"]
["BIMED","BM-22L"]
["BIMED","BM-23"]
["BIMED","BM-24"]
["BIMED","BM-25"]
["BIMED","BM-26"]
["BIMED","BM-27"]
["BIMED","BM-28"]
["BIMED","BM-29"]
["TECHNIK SPECIAL - AKCIA","BM-2A"]
["BIMED","BM-2S"]
["BIMED","BM-30"]
["BIMED","BMBC-01"]
["BIMED","BMBC-02"]
["BIMED","BMBC-03"]
["BIMED","BMBC-04"]
["BIMED","BMBC-05"]
["BIMED","BMBC-06"]
["BIMED","BMBC-07"]
["BIMED","BMBC-07S"]
["BIMED","BMBC-0S"]
["BIMED","BMBCVG-01"]
["BIMED","BMBCVG-01L"]
["BIMED","BMBCVG-02"]
["BIMED","BMBCVG-0S"]
["BIMED","BMBE-01"]
["BIMED","BMBE-02"]
["BIMED","BMBE-03"]
["BIMED","BMBE-04"]
["BIMED","BMBE-05"]
["BIMED","BMBE-06"]
["BIMED","BMBE-07"]
["BIMED","BMBE-0S"]
["BIMED","BMBL-01"]
["BIMED","BMBL-02"]
["BIMED","BMBL-03"]
["BIMED","BMBL-04"]
["BIMED","BMBL-05"]
["BIMED","BMBL-06"]
["BIMED","BMBL-07"]
["BIMED","BMBL-08"]
["BIMED","BMBL-09"]
["BIMED","BMBL-10"]
["BIMED","BMBL-10S"]
["BIMED","BMBL-11"]
["BIMED","BMBL-12"]
["BIMED","BMBL-13"]
["BIMED","BMBLS-01"]
["BIMED","BMBLS-02"]
["BIMED","BMBLS-03"]
["BIMED","BMBLS-04"]
["BIMED","BMBLS-05"]
["BIMED","BMBLS-06"]
["BIMED","BMBLS-07"]
["BIMED","BMBLS-08"]
["BIMED","BMBLS-09"]
["BIMED","BMBLS-10"]
["BIMED","BMBLS-11"]
["BIMED","BMBLS-12"]
["BIMED","BMBLS-13"]
["BIMED","BMBS-11"]
["BIMED","BMBS-12"]
["BIMED","BMBS-13"]
["BIMED","BMBS-14"]
["BIMED","BMBS-15"]
["BIMED","BMBS-16"]
["BIMED","BMBS-1S"]
["BIMED","BMBS-21"]
["BIMED","BMBS-22"]
["BIMED","BMBS-23"]
["BIMED","BMBS-24"]
["BIMED","BMBS-25"]
["BIMED","BMBS-26"]
["BIMED","BMBS-2S"]
["BIMED","BMEL-01"]
["BIMED","BMEL-02"]
["BIMED","BMEL-03"]
["BIMED","BMEL-04"]
["BIMED","BMEL-05"]
["BIMED","BMEL-06"]
["BIMED","BMEL-07"]
["BIMED","BMEL-08"]
["BIMED","BMEM-01"]
["BIMED","BMEM-02"]
["BIMED","BMEM-03"]
["BIMED","BMEM-04"]
["BIMED","BMEM-05"]
["BIMED","BMEM-06"]
["BIMED","BMEM-07"]
["BIMED","BMEM-0S"]
["BIMED","BMEN-01"]
["BIMED","BMEN-02"]
["BIMED","BMEN-03"]
["BIMED","BMEN-04"]
["BIMED","BMEN-05"]
["BIMED","BMEN-06"]
["BIMED","BMEN-07"]
["BIMED","BMEN-0S"]
["BIMED","BM-EN-11"]
["BIMED","BM-EN-12"]
["BIMED","BM-EN-13"]
["BIMED","BM-EN-14"]
["BIMED","BM-EN-15"]
["BIMED","BM-EN-16"]
["BIMED","BM-EN-17"]
["BIMED","BM-EN-1S"]
["BIMED","BML-01"]
["BIMED","BML-02"]
["BIMED","BML-03"]
["BIMED","BML-04"]
["BIMED","BML-05"]
["BIMED","BML-06"]
["BIMED","BML-07"]
["BIMED","BML-0S"]
["BIMED","BML-11"]
["BIMED","BML-12"]
["BIMED","BML-13"]
["BIMED","BML-14"]
["BIMED","BML-15"]
["BIMED","BML-16"]
["BIMED","BML-17"]
["BIMED","BML-1S"]
["BIMED","BML-21"]
["BIMED","BML-22"]
["BIMED","BML-23"]
["BIMED","BML-24"]
["BIMED","BML-25"]
["BIMED","BML-26"]
["BIMED","BML-27"]
["BIMED","BML-2S"]
["BIMED","BMOS-11"]
["BIMED","BMOS-12"]
["BIMED","BMSC-01"]
["BIMED","BMSC-02"]
["BIMED","BMSC-03"]
["BIMED","BMSC-04"]
["BIMED","BMSC-05"]
["BIMED","BMSC-06"]
["BIMED","BMSC-07"]
["BIMED","BMSC-0S"]
["BIMED","BMSP-11"]
["BIMED","BMSP-12"]
["BIMED","BMSP-12L"]
["BIMED","BMSP-13"]
["BIMED","BMSP-14"]
["BIMED","BMSP-15"]
["BIMED","BMSP-1S"]
["BIMED","BMSP-21"]
["BIMED","BMSP-22"]
["BIMED","BMSP-22L"]
["BIMED","BMSP-24"]
["BIMED","BMSP-25"]
["BIMED","BMSP-2S"]
["BIMED","BMVG-01"]
["BIMED","BMVG-02"]
["BIMED","BMVG-0S"]
["BIMED","BMVG-11"]
["BIMED","BMVG-12"]
["BIMED","BMVG-1S"]
["BIMED","BMVG-21"]
["BIMED","BMVG-22"]
["BIMED","BMVG-2S"]
["BIMED","BM-X0"]
["BIMED","BM-X1"]
["BIMED","BM-X1L"]
["BIMED","BM-X2"]
["BIMED","BM-X2L"]
["BIMED","BM-X3"]
["BIMED","BM-X4"]
["BIMED","BM-X5"]
["BIMED","BM-X6"]
["BIMED","BM-X7"]
["BIMED","BM-X8"]
["BIMED","BM-X9"]
["BIMED","BM-XS"]
["TECHNIK SPECIAL - AKCIA","BP 1"]
["TECHNIK SPECIAL - AKCIA","BP 3"]
["TECHNIK","BP 48x66 bílá"]
["TECHNIK","BP 48x66 bílá KŘEHKÉ"]
["TECHNIK","BP 48x66 hnědá"]
["TECHNIK","BP 48x66 transp"]
["ABTECH","BPG 1"]
["ABTECH","BPG 1.5"]
["ABTECH","BPG 10"]
["ABTECH","BPG 11"]
["ABTECH","BPG 12"]
["ABTECH","BPG 13"]
["ABTECH","BPG 13.5"]
["ABTECH","BPG 14"]
["ABTECH","BPG 15"]
["ABTECH","BPG 2"]
["ABTECH","BPG 2.5"]
["ABTECH","BPG 3"]
["ABTECH","BPG 3.5"]
["ABTECH","BPG 4"]
["ABTECH","BPG 4.5"]
["ABTECH","BPG 5"]
["ABTECH","BPG 6"]
["ABTECH","BPG 7"]
["ABTECH","BPG 8"]
["ABTECH","BPG 9"]
["ABTECH","BPG-EX 1"]
["ABTECH","BPG-EX 10"]
["ABTECH","BPG-EX 11"]
["ABTECH","BPG-EX 12"]
["ABTECH","BPG-EX 13"]
["ABTECH","BPG-EX 13.5"]
["ABTECH","BPG-EX 14"]
["ABTECH","BPG-EX 15"]
["ABTECH","BPG-EX 2"]
["ABTECH","BPG-EX 3"]
["ABTECH","BPG-EX 4"]
["ABTECH","BPG-EX 4.5"]
["ABTECH","BPG-EX 5"]
["ABTECH","BPG-EX 6"]
["ABTECH","BPG-EX 7"]
["ABTECH","BPG-EX 8"]
["ABTECH","BPG-EX 9"]
["TECHNIK SPECIAL - AKCIA","BPS 230.14"]
["TECHNIK SPECIAL - AKCIA","BPS 230.24"]
["BIMED","BPT-21/BPM-2S"]
["BIMED","BPT-22/BPM-E21"]
["BIMED","BPT-23/BPM-21"]
["BIMED","BPT-24/BPM-22"]
["BIMED","BPT-25/BPM-22L"]
["BIMED","BPT-26/BPM-E23"]
["BIMED","BPT-27/BPM-24"]
["BIMED","BPT-28/BPM-E25"]
["BIMED","BPT-29/BPM-26"]
["BIMED","BPT-30/BPM-27"]
["TECHNIK","Brašna M"]
["TECHNIK","Brašna V"]
["TECHNIK SPECIAL - AKCIA","BS 160"]
["TECHNIK SPECIAL - AKCIA","BS 160/R5"]
["BIMED","BS-01"]
["BIMED","BS-02"]
["BIMED","BS-03"]
["BIMED","BS-04"]
["BIMED","BS-05"]
["BIMED","BS-06"]
["BIMED","BS-07"]
["BIMED","BS-08"]
["BIMED","BS-09"]
["BIMED","BS-10"]
["BIMED","BS-11"]
["BIMED","BS-12"]
["BIMED","BS-13"]
["BIMED","BS-14"]
["BIMED","BS-15"]
["BIMED","BS-16"]
["BIMED","BS-17"]
["BIMED","BS-18"]
["BIMED","BS-19"]
["BIMED","BS-20"]
["BIMED","BS-21"]
["BIMED","BS-22"]
["BIMED","BS-23"]
["BIMED","BS-24"]
["BIMED","BS-25"]
["BIMED","BS-26"]
["BIMED","BS-27"]
["BIMED","BS-28"]
["BIMED","BS-29"]
["BIMED","BS-30"]
["BIMED","BSBC-01"]
["BIMED","BSBC-02"]
["BIMED","BSBC-03"]
["BIMED","BSBC-04"]
["BIMED","BSBC-05"]
["BIMED","BSBC-06"]
["BIMED","BSBC-07"]
["BIMED","BSBC-08"]
["BIMED","BSBC-09"]
["BIMED","BSBC-10"]
["BIMED","BSBCVG-01"]
["BIMED","BSBCVG-02"]
["BIMED","BSBCVG-03"]
["BIMED","BSBCVG-04"]
["BIMED","BSBE-01"]
["BIMED","BSBE-02"]
["BIMED","BSBE-03"]
["BIMED","BSBE-04"]
["BIMED","BSBE-05"]
["BIMED","BSBE-06"]
["BIMED","BSBE-07"]
["BIMED","BSBE-08"]
["BIMED","BSBE-09"]
["BIMED","BSBE-10"]
["BIMED","BSEL-01"]
["BIMED","BSEL-02"]
["BIMED","BSEL-03"]
["BIMED","BSEL-04"]
["BIMED","BSEL-05"]
["BIMED","BSEL-06"]
["BIMED","BSEL-07"]
["BIMED","BSEL-08"]
["BIMED","BSEL-09"]
["BIMED","BSEL-10"]
["BIMED","BSEM-01"]
["BIMED","BSEM-02"]
["BIMED","BSEM-03"]
["BIMED","BSEM-04"]
["BIMED","BSEM-05"]
["BIMED","BSEM-06"]
["BIMED","BSEM-07"]
["BIMED","BSEM-08"]
["BIMED","BSEM-09"]
["BIMED","BSEM-10"]
["BIMED","BSEN-01"]
["BIMED","BSEN-02"]
["BIMED","BSEN-03"]
["BIMED","BSEN-04"]
["BIMED","BSEN-05"]
["BIMED","BSEN-06"]
["BIMED","BSEN-07"]
["BIMED","BSL-01"]
["BIMED","BSL-02"]
["BIMED","BSL-03"]
["BIMED","BSL-04"]
["BIMED","BSL-05"]
["BIMED","BSL-06"]
["BIMED","BSL-07"]
["BIMED","BSL-08"]
["BIMED","BSL-09"]
["BIMED","BSL-10"]
["BIMED","BSLS-01"]
["BIMED","BSLS-02"]
["BIMED","BSLS-03"]
["BIMED","BSLS-04"]
["BIMED","BSLS-05"]
["BIMED","BSLS-06"]
["BIMED","BSLS-07"]
["BIMED","BSLS-08"]
["BIMED","BSLS-09"]
["BIMED","BSLS-10"]
["BIMED","BSSC-01"]
["BIMED","BSSC-02"]
["BIMED","BSSC-03"]
["BIMED","BSSC-04"]
["BIMED","BSSC-05"]
["BIMED","BSSC-06"]
["BIMED","BSSC-07"]
["BIMED","BSSC-08"]
["BIMED","BSSC-09"]
["BIMED","BSSC-10"]
["BIMED","BSSP-11"]
["BIMED","BSSP-12"]
["BIMED","BSSP-13"]
["BIMED","BSSP-14"]
["BIMED","BSSP-15"]
["BIMED","BSSP-16"]
["BIMED","BSSP-21"]
["BIMED","BSSP-22"]
["BIMED","BSSP-23"]
["BIMED","BSSP-24"]
["BIMED","BSSP-25"]
["BIMED","BSSP-26"]
["BIMED","BSVG-02"]
["BIMED","BSVG-04"]
["BIMED","BSVG-12"]
["BIMED","BSVG-14"]
["BIMED","BSVG-22"]
["BIMED","BSVG-24"]
["TECHNIK SPECIAL - AKCIA","B-TC 026"]
["TECHNIK SPECIAL - AKCIA","B-TC 04"]
["TECHNIK SPECIAL - AKCIA","B-TC 051"]
["TECHNIK SPECIAL - AKCIA","B-TC 055"]
["TECHNIK SPECIAL - AKCIA","B-TC 065"]
["TECHNIK SPECIAL - AKCIA","B-TC 095"]
["TECHNIK SPECIAL - AKCIA","B-TC 650"]
["BIMED","BVPA-11"]
["BIMED","BVPA-21"]
["BIMED","BVPB-11"]
["BIMED","BVPB-11L"]
["BIMED","BVPB-21"]
["BIMED","BVPB-21L"]
["TECHNIK SPECIAL - AKCIA","BW 200"]
["TECHNIK","BZ 44F"]
["TECHNIK","BZ 44F pružina"]
["TECHNIK","BZ 4500HS"]
["TECHNIK","C. 1695-M10"]
["TECHNIK","C. 1695-M12"]
["TECHNIK","C. 50150-M12"]
["TECHNIK","C. 50150-M16"]
["TECHNIK","C. 95240-M12"]
["TECHNIK","C. 95240-M16"]
["TECHNIK","C.120300-M12"]
["TECHNIK","C.120300-M16"]
["TECHNIK","C.185400-M16"]
["TECHNIK SPECIAL - AKCIA","C15-SK 014"]
["TECHNIK","C1-BP 051"]
["TECHNIK","C1-BP 1525"]
["TECHNIK","C1-D 0256"]
["TECHNIK","C1-D 1025"]
["TECHNIK","C1-D 3550"]
["TECHNIK","C1-DD 616"]
["TECHNIK","C1-DSK 08056"]
["TECHNIK","C1-H&S 4"]
["TECHNIK","C1-H&S 6"]
["TECHNIK","C1-HIR"]
["TECHNIK","C1-KK 01415"]
["TECHNIK","C1-MC 3"]
["TECHNIK","C1-MC 4"]
["TECHNIK","C1-MC 4/4 UNI"]
["TECHNIK","C1-MC 4/6 UNI"]
["TECHNIK","C1-MK 0525"]
["TECHNIK","C1-MO 0125"]
["TECHNIK","C1-MO 054"]
["TECHNIK","C1-MO 056"]
["TECHNIK","C1-OI 056"]
["TECHNIK","C1-OI 1016"]
["TECHNIK","C1-OL 1510"]
["TECHNIK","C1-ON 02525"]
["TECHNIK","C1-ON 0510"]
["TECHNIK","C1-ON 1625"]
["TECHNIK","C1-ON 410"]
["TECHNIK","C1-SIS 056"]
["TECHNIK","C1-SK 0144"]
["TECHNIK","C1-SK 156"]
["TECHNIK","C1-SK 410"]
["TECHNIK","C1-T 468W"]
["TECHNIK","C1-TYCO"]
["TECHNIK","C1-X 1"]
["TECHNIK","C1-X 2"]
["TECHNIK","C1-X 5"]
["TECHNIK","C2-BP 0525"]
["TECHNIK","C2-D 02516"]
["TECHNIK","C2-D 0516"]
["TECHNIK","C2-D 054"]
["TECHNIK","C2-D 056"]
["TECHNIK","C2-D 1635"]
["TECHNIK","C2-D 25/50"]
["TECHNIK","C2-D 35"]
["TECHNIK","C2-D 50"]
["TECHNIK","C2-D 616"]
["TECHNIK","C2-DSK 05075"]
["TECHNIK","C2-DSK 0805"]
["TECHNIK","C2-FO SMA"]
["TECHNIK","C2-FO ST"]
["TECHNIK","C2-KK 02515"]
["TECHNIK","C2-MC 3H"]
["TECHNIK","C2-MC 3T"]
["TECHNIK","C2-MC 4H"]
["TECHNIK","C2-MC 4T"]
["TECHNIK","C2-MO 0525"]
["TECHNIK","C2-MO 0525 BP"]
["TECHNIK","C2-MO 0525 BP-B"]
["TECHNIK","C2-MO 056"]
["TECHNIK","C2-OI 056"]
["TECHNIK","C2-OL 056"]
["TECHNIK","C2-ON 0510"]
["TECHNIK","C2-ON 07510"]
["TECHNIK","C2-ON 1025"]
["TECHNIK","C2-SIS 056"]
["TECHNIK","C2-SK 156"]
["TECHNIK","C2-T10"]
["TECHNIK","C2-T4"]
["TECHNIK","C2-T6"]
["TECHNIK","C2-T68"]
["TECHNIK","C2-T6A"]
["TECHNIK","C2-T6DEC"]
["TECHNIK","C2-T8"]
["TECHNIK","C2-T8A"]
["TECHNIK","C2-T8H"]
["TECHNIK","C2-T8M5"]
["TECHNIK","C2-T8M6"]
["TECHNIK","C2-T8Q"]
["TECHNIK","C2-T8S"]
["TECHNIK","C2-X 1"]
["TECHNIK","C2-X 2"]
["TECHNIK","C2-X 3"]
["TECHNIK","C2-X 4"]
["TECHNIK","C2-X 5"]
["TECHNIK","C2-X 6"]
["TECHNIK","C2-X 7"]
["TECHNIK","C2-X 8"]
["TECHNIK","C2-X 9"]
["TECHNIK SPECIAL - AKCIA","C3-BP 0515"]
["TECHNIK SPECIAL - AKCIA","C3-BP 1525"]
["TECHNIK SPECIAL - AKCIA","C3-BPI 1525"]
["TECHNIK SPECIAL - AKCIA","C3-D 01425"]
["TECHNIK SPECIAL - AKCIA","C3-D 0256"]
["TECHNIK SPECIAL - AKCIA","C3-D 2535"]
["TECHNIK SPECIAL - AKCIA","C3-D 2550"]
["TECHNIK SPECIAL - AKCIA","C3-D 616"]
["TECHNIK SPECIAL - AKCIA","C3-MO 01415"]
["TECHNIK SPECIAL - AKCIA","C3-MO 056"]
["TECHNIK SPECIAL - AKCIA","C3-OI 02525"]
["TECHNIK SPECIAL - AKCIA","C3-OI 056"]
["TECHNIK SPECIAL - AKCIA","C3-OL 156"]
["TECHNIK SPECIAL - AKCIA","C3-ON 056"]
["TECHNIK SPECIAL - AKCIA","C3-ON10"]
["TECHNIK SPECIAL - AKCIA","C3-ON16"]
["TECHNIK SPECIAL - AKCIA","C3-PT"]
["TECHNIK SPECIAL - AKCIA","C3-SK 0525"]
["TECHNIK SPECIAL - AKCIA","C3-SK 0754"]
["TECHNIK SPECIAL - AKCIA","C3-X1"]
["TECHNIK SPECIAL - AKCIA","C3-X2"]
["TECHNIK SPECIAL - AKCIA","C4-BP 0515B"]
["TECHNIK SPECIAL - AKCIA","C4-BP 0575"]
["TECHNIK SPECIAL - AKCIA","C4-BP 115"]
["TECHNIK SPECIAL - AKCIA","C4-BPI 1525"]
["TECHNIK SPECIAL - AKCIA","C4-D 0086"]
["TECHNIK SPECIAL - AKCIA","C4-D 1025"]
["TECHNIK SPECIAL - AKCIA","C4-D 3550"]
["TECHNIK SPECIAL - AKCIA","C4-DD 410"]
["TECHNIK SPECIAL - AKCIA","C4-MC3"]
["TECHNIK SPECIAL - AKCIA","C4-MO 0115"]
["TECHNIK SPECIAL - AKCIA","C4-MO 056"]
["TECHNIK SPECIAL - AKCIA","C4-OI 0115"]
["TECHNIK SPECIAL - AKCIA","C4-OI 01425"]
["TECHNIK SPECIAL - AKCIA","C4-OI 02525"]
["TECHNIK SPECIAL - AKCIA","C4-OI 056"]
["TECHNIK SPECIAL - AKCIA","C4-OI 056PA"]
["TECHNIK SPECIAL - AKCIA","C4-OI 056PC"]
["TECHNIK SPECIAL - AKCIA","C4-OL 03425"]
["TECHNIK SPECIAL - AKCIA","C4-OL 410"]
["TECHNIK SPECIAL - AKCIA","C4-ON 02525"]
["TECHNIK SPECIAL - AKCIA","C4-ON 0510"]
["TECHNIK SPECIAL - AKCIA","C4-ON 16"]
["TECHNIK SPECIAL - AKCIA","C4-SK 0144"]
["TECHNIK SPECIAL - AKCIA","C4-SK 610"]
["TECHNIK SPECIAL - AKCIA","C6-OI 0525"]
["TECHNIK SPECIAL - AKCIA","C6-ON 410"]
["TECHNIK","CCB 2 - 33/14"]
["TECHNIK","CCB 2 - 50/21"]
["TECHNIK","CCB 2 - 98/28"]
["TECHNIK","CCB 3 - 25/9"]
["TECHNIK","CCB 3 - 38/11"]
["TECHNIK","CCB 3 - 60/24"]
["TECHNIK","CCB 3 - 80/36"]
["TECHNIK","CCB 3 -100/48"]
["TECHNIK","CCB 3 -125/55"]
["TECHNIK","CCB 3 -140/70"]
["TECHNIK","CCB 4 - 28/9"]
["TECHNIK","CCB 4 - 38/11"]
["TECHNIK","CCB 4 - 55/20"]
["TECHNIK","CCB 4 - 75/25"]
["TECHNIK","CCB 4 -100/35"]
["TECHNIK","CCB 4 -125/45"]
["TECHNIK","CCB 5 - 38/12"]
["TECHNIK","CCB 5 - 53/15"]
["TECHNIK","CCB 5 - 80/26"]
["TECHNIK","CCB 5 -102/34"]
["TECHNIK","CC-D 0510"]
["TECHNIK","CC-D 1635"]
["TECHNIK","CC-MO 056"]
["TECHNIK","CC-OI 056"]
["TECHNIK","CC-ON 0510"]
["TECHNIK","CC-T6"]
["TECHNIK","CC-T8C"]
["TECHNIK","CC-T8H"]
["TECHNIK","CC-T8S"]
["TECHNIK","CC-X 1"]
["TECHNIK","CFM   8/2 A"]
["TECHNIK","CFM   9/3 A"]
["TECHNIK","CFM  12/4 A"]
["TECHNIK","CFM  16/5 A"]
["TECHNIK","CFM  19/6 A"]
["TECHNIK","CFM  22/6 A"]
["TECHNIK","CFM  25/8 A"]
["TECHNIK","CFM  28/9 A"]
["TECHNIK","CFM  33/11 A"]
["TECHNIK","CFM  40/12 A"]
["TECHNIK","CFM  43/13 A"]
["TECHNIK","CFM  55/16 A"]
["TECHNIK","CFM  65/19 A"]
["TECHNIK","CFM  75/22 A"]
["TECHNIK","CFM  85/25 A"]
["TECHNIK","CFM  95/25 A"]
["TECHNIK","CFM 115/34 A"]
["TECHNIK","CFM 140/42 A"]
["TECHNIK","CFM 160/50 A"]
["TECHNIK","CFM 175/58 A"]
["TECHNIK","CFM 210/65 A"]
["TECHNIK","CFM 230/75 A"]
["TECHNIK","CFW   9/3 A"]
["TECHNIK","CFW  12/4 A"]
["TECHNIK","CFW  33/8 A"]
["TECHNIK","CFW  45/13 A"]
["TECHNIK","CFW  55/16 A"]
["TECHNIK","CFW  65/19 A"]
["TECHNIK","CFW  75/22 A"]
["TECHNIK","CFW  85/25 A"]
["TECHNIK","CFW  95/30 A"]
["TECHNIK","CFW 105/30 A"]
["TECHNIK","CFW 115/34 A"]
["TECHNIK","CFW 140/42 A"]
["TECHNIK","CFW 175/50 A"]
["TECHNIK","CFW 200/60 A"]
["TECHNIK","CIM 12 0500"]
["TECHNIK","CLEAR GLIDE"]
["TECHNIK","CM 1"]
["TECHNIK","CM 1-1"]
["TECHNIK","CM 1-2"]
["TECHNIK","CM 1-3"]
["TECHNIK","CM 2"]
["TECHNIK SPECIAL - AKCIA","CM 25 - KA 11"]
["TECHNIK SPECIAL - AKCIA","CM 25-3"]
["TECHNIK SPECIAL - AKCIA","CM 25-3-0146"]
["TECHNIK","CM 3"]
["TECHNIK","CM 4"]
["TECHNIK","CM 5"]
["TECHNIK","CM 5-1"]
["TECHNIK","CM 6"]
["TECHNIK","CM 7"]
["TECHNIK","CM 8"]
["TECHNIK","CM 9"]
["TECHNIK","COAX-STRIP  8"]
["TECHNIK","COAX-STRIP 12"]
["TECHNIK","COAX-STRIP 12/3"]
["TECHNIK","COAX-STRIP 12/6"]
["TECHNIK","COAX-STRIP UNI"]
["TECHNIK","Cockpit sprej"]
["TECHNIK","COM 2/0"]
["TECHNIK","COM 2/1"]
["TECHNIK","COM 2/2"]
["TECHNIK","COM 2/3"]
["TECHNIK","COM 2/4"]
["TECHNIK","COM 2/5"]
["TECHNIK","COM 2/6"]
["TECHNIK","COM 2/7"]
["TECHNIK","COM 2/8"]
["TECHNIK","COM 2/9"]
["TECHNIK","COM 2/E"]
["TECHNIK","COM 2/L"]
["TECHNIK","COM 2/N"]
["TECHNIK","COM 2/P"]
["TECHNIK","COM 2/zem"]
["TECHNIK","COM 3/0"]
["TECHNIK","COM 3/1"]
["TECHNIK","COM 3/2"]
["TECHNIK","COM 3/3"]
["TECHNIK","COM 3/4"]
["TECHNIK","COM 3/5"]
["TECHNIK","COM 3/6"]
["TECHNIK","COM 3/7"]
["TECHNIK","COM 3/8"]
["TECHNIK","COM 3/9"]
["TECHNIK","COM 3/A"]
["TECHNIK","COM 3/C"]
["TECHNIK","COM 3/G"]
["TECHNIK","COM 3/L"]
["TECHNIK","COM 3/N"]
["TECHNIK","COM 3/P"]
["TECHNIK","COM 3/R"]
["TECHNIK","COM 3/S"]
["TECHNIK","COM 3/T"]
["TECHNIK","COM 4/0"]
["TECHNIK","COM 4/1"]
["TECHNIK","COM 4/2"]
["TECHNIK","COM 4/3"]
["TECHNIK","COM 4/4"]
["TECHNIK","COM 4/5"]
["TECHNIK","COM 4/6"]
["TECHNIK","COM 4/7"]
["TECHNIK","COM 4/8"]
["TECHNIK","COM 4/9"]
["TECHNIK","COM 5/0"]
["TECHNIK","COM 5/1"]
["TECHNIK","COM 5/2"]
["TECHNIK","COM 5/3"]
["TECHNIK","COM 5/4"]
["TECHNIK","COM 5/5"]
["TECHNIK","COM 5/6"]
["TECHNIK","COM 5/7"]
["TECHNIK","COM 5/8"]
["TECHNIK","COM 5/9"]
["TECHNIK","COM 6/0"]
["TECHNIK","COM 6/1"]
["TECHNIK","COM 6/2"]
["TECHNIK","COM 6/3"]
["TECHNIK","COM 6/4"]
["TECHNIK","COM 6/5"]
["TECHNIK","COM 6/6"]
["TECHNIK","COM 6/7"]
["TECHNIK","COM 6/8"]
["TECHNIK","COM 6/9"]
["TECHNIK","COM 6/A"]
["TECHNIK","COM 6/B"]
["TECHNIK","COM 6/C"]
["TECHNIK","COM 6/M"]
["TECHNIK","COM 6/S"]
["TECHNIK","COM 6/W"]
["TECHNIK","COM 6/X"]
["TECHNIK","COM 9/1"]
["TECHNIK","COM 9/2"]
["TECHNIK","COM 9/3"]
["TECHNIK","COM 9/E"]
["TECHNIK","COM 9/P"]
["TECHNIK","COM 9/T"]
["TECHNIK SPECIAL - AKCIA","COMBI"]
["TECHNIK SPECIAL - AKCIA","COMBI SET"]
["TECHNIK SPECIAL - AKCIA","COMBI SET M16-40"]
["TECHNIK SPECIAL - AKCIA","COMBI SET M16-63"]
["TECHNIK SPECIAL - AKCIA","COMBI SET Pg9-48"]
["TECHNIK SPECIAL - AKCIA","COMBI SET+ M16-40"]
["TECHNIK SPECIAL - AKCIA","COMBI SET+ M16-63"]
["TECHNIK SPECIAL - AKCIA","COMBI SET+ Pg9-42"]
["TECHNIK SPECIAL - AKCIA","COMBI STD Pg7-48"]
["TECHNIK SPECIAL - AKCIA","COMPACT"]
["TECHNIK SPECIAL - AKCIA","COMPACT FLEX"]
["TECHNIK SPECIAL - AKCIA","COMPACT FLEX SET"]
["TECHNIK SPECIAL - AKCIA","COMPACT kufr"]
["TECHNIK SPECIAL - AKCIA","COMPACT SET"]
["TECHNIK SPECIAL - AKCIA","COMPACT SET M16-40"]
["TECHNIK SPECIAL - AKCIA","COMPACT SET M16-63"]
["TECHNIK SPECIAL - AKCIA","COMPACT SET Pg9-48"]
["TECHNIK SPECIAL - AKCIA","COMPACT SET+ M16-40"]
["TECHNIK SPECIAL - AKCIA","COMPACT SET+ M16-63"]
["TECHNIK SPECIAL - AKCIA","COMPACT SET+ Pg9-42"]
["TECHNIK SPECIAL - AKCIA","COMPACT STD Pg9-42"]
["TECHNIK SPECIAL - AKCIA","COMPACT těsnění"]
["TECHNIK","Corro ochrana sprej"]
["TECHNIK","COSSONAY I"]
["TECHNIK","COSSONAY II"]
["TECHNIK","CPA300  3/1"]
["TECHNIK","CPA300  6,4/2,0"]
["TECHNIK","CPA300 12,7/4,1"]
["TECHNIK","CPA300 19/7,5"]
["TECHNIK SPECIAL - AKCIA","CRIMPER-G"]
["TECHNIK SPECIAL - AKCIA","CRIMPER-L"]
["TECHNIK","CRIMPIT F 4"]
["TECHNIK","CRIMPIT F 6auto"]
["TECHNIK","CRIMPIT F 6gyra"]
["TECHNIK","CRIMPIT F 6L"]
["TECHNIK","CRIMPIT F16L"]
["TECHNIK","CRIMPIT F25L"]
["TECHNIK","CRIMPIT F50EN"]
["TECHNIK","CRIMPIT F50L"]
["TECHNIK","CRIMPIT IT6L"]
["TECHNIK","CRIMPIT IT6S"]
["TECHNIK SPECIAL - AKCIA","CS 60"]
["TECHNIK","C-SCORA  2T"]
["TECHNIK","C-SCORA  6T"]
["TECHNIK","C-SCORA 10T"]
["TECHNIK","C-SCORA 16T"]
["TECHNIK","C-SCORA 25T"]
["TECHNIK","C-SCORA 2x1/4,8/6,6"]
["TECHNIK","C-SCORA 6Tsolar"]
["TECHNIK","C-SCORA 708216"]
["TECHNIK","C-SCORA 708245"]
["TECHNIK","C-SCORA 8,9"]
["TECHNIK","Cupal 0,5x500x2000"]
["TECHNIK","Cupal 1,0x500x2000"]
["TECHNIK","Cupal 1,5x500x2000"]
["TECHNIK","Cupal 2,0x500x2000"]
["TECHNIK","Cupal 25x100"]
["TECHNIK","Cupal 50x 3"]
["TECHNIK","Cupal 50x 4"]
["TECHNIK","Cupal 50x 4/0,5"]
["TECHNIK","Cupal 50x 5"]
["TECHNIK","Cupal 50x 6"]
["TECHNIK","Cupal 50x 6/0,5"]
["TECHNIK","Cupal 50x 8"]
["TECHNIK","Cupal 50x 8/0,5"]
["TECHNIK","Cupal 50x10"]
["TECHNIK","Cupal 50x10/0,5"]
["TECHNIK","Cupal 50x100"]
["TECHNIK","Cupal 50x11"]
["TECHNIK","Cupal 50x12"]
["TECHNIK","Cupal 50x17,5"]
["TECHNIK","Cupal 50x20"]
["TECHNIK","Cupal 50x25"]
["TECHNIK","Cupal 50x30"]
["TECHNIK","Cupal 50x50"]
["TECHNIK","Cupal 50x50/0,5"]
["TECHNIK","Cupal M 3"]
["TECHNIK","Cupal M 4"]
["TECHNIK","Cupal M 5"]
["TECHNIK","Cupal M 5/2"]
["TECHNIK","Cupal M 6"]
["TECHNIK","Cupal M 6/2"]
["TECHNIK","Cupal M 8"]
["TECHNIK","Cupal M 8/2"]
["TECHNIK","Cupal M10"]
["TECHNIK","Cupal M10/2"]
["TECHNIK","Cupal M12"]
["TECHNIK","Cupal M12/2"]
["TECHNIK","Cupal M14"]
["TECHNIK","Cupal M14/2"]
["TECHNIK","Cupal M16"]
["TECHNIK","Cupal M16/2"]
["TECHNIK","Cupal M20"]
["TECHNIK","Cupal M20/2"]
["TECHNIK","CV-KC 1"]
["TECHNIK","CV-KC 2"]
["TECHNIK","CV-KC 3"]
["TECHNIK","CV-KC 4"]
["TECHNIK","CV-KC 5"]
["TECHNIK","CV-KC 6"]
["TECHNIK","CV-KC 7"]
["TECHNIK","CV-KC 8"]
["TECHNIK","CV-KC11"]
["TECHNIK","CV-KC13"]
["TECHNIK","CV-KC15"]
["TECHNIK","CV-KC17"]
["TECHNIK","CV-KC18"]
["TECHNIK","CV-KC19"]
["TECHNIK","CV-KC20"]
["TECHNIK","Čepel A"]
["TECHNIK","Čepel H"]
["TECHNIK","Čepel L"]
["TECHNIK","Čepel ODL  9"]
["TECHNIK","Čepel ODL 18"]
["TECHNIK","Čepel ODL-BM 18"]
["TECHNIK","Čepel ODL-BM 18/50"]
["TECHNIK","Čepel T"]
["TECHNIK","Čepel T-BM"]
["TECHNIK","Čistič brzd"]
["TECHNIK","Čistič el. kontaktů"]
["TECHNIK","Čistič hořáků"]
["TECHNIK","Čistič plastů sprej"]
["TECHNIK","Čistič S sprej"]
["TECHNIK","D 150240"]
["TECHNIK","D 70150"]
["TECHNIK","DATA-STRIP"]
["TECHNIK","DBKPH-SET"]
["TECHNIK","DD  0,25-8 fialová"]
["TECHNIK","DD  0,25-8 modrá"]
["TECHNIK","DD  0,25-8 modrá 100"]
["TECHNIK","DD  0,34-8 tyrkys100"]
["TECHNIK","DD  0,34-8 tyrkysová"]
["TECHNIK","DD  0,5- 6 bílá"]
["TECHNIK","DD  0,5- 6 oranž 100"]
["TECHNIK","DD  0,5- 6 oranžová"]
["TECHNIK","DD  0,5- 8 bílá"]
["TECHNIK","DD  0,5- 8 bílá 100"]
["TECHNIK","DD  0,5- 8 oranž 100"]
["TECHNIK","DD  0,5- 8 oranžová"]
["TECHNIK","DD  0,5-10 bílá"]
["TECHNIK","DD  0,5-10 bílá 100"]
["TECHNIK","DD  0,5-10 oranžová"]
["TECHNIK","DD  0,5-12 bílá"]
["TECHNIK","DD  0,5-12 oranž 100"]
["TECHNIK","DD  0,5-12 oranžová"]
["TECHNIK","DD  0,75- 8 bílá"]
["TECHNIK","DD  0,75- 8 bílá 100"]
["TECHNIK","DD  0,75- 8 modrá"]
["TECHNIK","DD  0,75- 8 modrá100"]
["TECHNIK","DD  0,75- 8 šedá"]
["TECHNIK","DD  0,75- 8 šedá 100"]
["TECHNIK","DD  0,75-10 bílá"]
["TECHNIK","DD  0,75-10 bílá 100"]
["TECHNIK","DD  0,75-10 modrá"]
["TECHNIK","DD  0,75-10 šedá"]
["TECHNIK","DD  0,75-12 bílá"]
["TECHNIK","DD  0,75-12 bílá 100"]
["TECHNIK","DD  0,75-12 modrá"]
["TECHNIK","DD  0,75-12 šedá"]
["TECHNIK","DD  0,75-18 bílá"]
["TECHNIK","DD  0,75-18 bílá 100"]
["TECHNIK","DD  1,0- 8 rudá"]
["TECHNIK","DD  1,0- 8 rudá 100"]
["TECHNIK","DD  1,0- 8 žlutá"]
["TECHNIK","DD  1,0- 8 žlutá 100"]
["TECHNIK","DD  1,0-10 rudá"]
["TECHNIK","DD  1,0-10 rudá 100"]
["TECHNIK","DD  1,0-10 žlutá"]
["TECHNIK","DD  1,0-10 žlutá 100"]
["TECHNIK","DD  1,0-12 rudá"]
["TECHNIK","DD  1,0-12 rudá 100"]
["TECHNIK","DD  1,0-12 žlutá"]
["TECHNIK","DD  1,0-12 žlutá 100"]
["TECHNIK","DD  1,0-18 rudá"]
["TECHNIK","DD  1,0-18 žlutá"]
["TECHNIK","DD  1,0-18 žlutá 100"]
["TECHNIK","DD  1,5- 8 černá"]
["TECHNIK","DD  1,5- 8 černá 100"]
["TECHNIK","DD  1,5- 8 rudá"]
["TECHNIK","DD  1,5- 8 rudá 100"]
["TECHNIK","DD  1,5-12 černá"]
["TECHNIK","DD  1,5-12 černá 100"]
["TECHNIK","DD  1,5-12 rudá"]
["TECHNIK","DD  1,5-12 rudá 100"]
["TECHNIK","DD  1,5-18 černá"]
["TECHNIK","DD  1,5-18 rudá"]
["TECHNIK","DD  2,5-10 modrá"]
["TECHNIK","DD  2,5-10 modrá 100"]
["TECHNIK","DD  2,5-10 šedá"]
["TECHNIK","DD  2,5-10 šedá 100"]
["TECHNIK","DD  2,5-13 modrá"]
["TECHNIK","DD  2,5-13 modrá 100"]
["TECHNIK","DD  2,5-13 šedá"]
["TECHNIK","DD  2,5-18 modrá"]
["TECHNIK","DD  2,5-18 šedá"]
["TECHNIK","DD  4-12 oranžová"]
["TECHNIK","DD  4-12 šedá"]
["TECHNIK","DD  4-18 šedá"]
["TECHNIK","DD  6-14 černá"]
["TECHNIK","DD  6-14 zelená"]
["TECHNIK","DD  6-14 žlutá"]
["TECHNIK","DD  6-18 černá"]
["TECHNIK","DD  6-18 žlutá"]
["TECHNIK","DD 10-14 hnědá"]
["TECHNIK","DD 10-14 rudá"]
["TECHNIK","DD 10-14 sl. kost"]
["TECHNIK","DD 10-18 sl. kost"]
["TECHNIK","DD 16-14 bílá"]
["TECHNIK","DD 16-14 modrá"]
["TECHNIK","DD 16-14 zelená"]
["TECHNIK","DD 16-16 zelená"]
["TECHNIK","DD 16-25 zelená"]
["TECHNIK","DI  0,14- 6 hnědá"]
["TECHNIK","DI  0,14- 6 hnědá100"]
["TECHNIK","DI  0,14- 6 šedá"]
["TECHNIK","DI  0,14- 6 šedá 100"]
["TECHNIK","DI  0,14- 8 hnědá"]
["TECHNIK","DI  0,14- 8 hnědá100"]
["TECHNIK","DI  0,14- 8 šedá"]
["TECHNIK","DI  0,14- 8 šedá 100"]
["TECHNIK","DI  0,25- 6 fialová"]
["TECHNIK","DI  0,25- 6 modrá"]
["TECHNIK","DI  0,25- 6 modrá100"]
["TECHNIK","DI  0,25- 6 žlutá"]
["TECHNIK","DI  0,25- 8 fial.100"]
["TECHNIK","DI  0,25- 8 fialová"]
["TECHNIK","DI  0,25- 8 modrá"]
["TECHNIK","DI  0,25- 8 modrá100"]
["TECHNIK","DI  0,25- 8 žlutá"]
["TECHNIK","DI  0,25- 8 žlutá100"]
["TECHNIK","DI  0,25-12 fialová"]
["TECHNIK","DI  0,25-12 modrá"]
["TECHNIK","DI  0,34- 6 růžová"]
["TECHNIK","DI  0,34- 6 tyrk 100"]
["TECHNIK","DI  0,34- 6 tyrkys."]
["TECHNIK","DI  0,34- 6 zelená"]
["TECHNIK","DI  0,34- 6 žlutá"]
["TECHNIK","DI  0,34- 8 růžo 100"]
["TECHNIK","DI  0,34- 8 růžová"]
["TECHNIK","DI  0,34- 8 tyrk 100"]
["TECHNIK","DI  0,34- 8 tyrkys."]
["TECHNIK","DI  0,34- 8 zele 100"]
["TECHNIK","DI  0,34- 8 zelená"]
["TECHNIK","DI  0,34- 8 žlutá"]
["TECHNIK","DI  0,34-12 růžová"]
["TECHNIK","DI  0,34-12 tyrkys."]
["TECHNIK","DI  0,5- 6 bílá"]
["TECHNIK","DI  0,5- 6 bílá 100"]
["TECHNIK","DI  0,5- 6 oranž 100"]
["TECHNIK","DI  0,5- 6 oranžová"]
["TECHNIK","DI  0,5- 8 bílá"]
["TECHNIK","DI  0,5- 8 bílá 100"]
["TECHNIK","DI  0,5- 8 oranž 100"]
["TECHNIK","DI  0,5- 8 oranžová"]
["TECHNIK","DI  0,5-10 bílá"]
["TECHNIK","DI  0,5-10 bílá 100"]
["TECHNIK","DI  0,5-10 oranž 100"]
["TECHNIK","DI  0,5-10 oranžová"]
["TECHNIK","DI  0,5-12 bílá"]
["TECHNIK","DI  0,5-12 oranž 100"]
["TECHNIK","DI  0,5-12 oranžová"]
["TECHNIK","DI  0,75- 6 bílá"]
["TECHNIK","DI  0,75- 6 bílá 100"]
["TECHNIK","DI  0,75- 6 modrá"]
["TECHNIK","DI  0,75- 6 šedá"]
["TECHNIK","DI  0,75- 6 šedá 100"]
["TECHNIK","DI  0,75- 8 bílá"]
["TECHNIK","DI  0,75- 8 bílá 100"]
["TECHNIK","DI  0,75- 8 modrá"]
["TECHNIK","DI  0,75- 8 modrá100"]
["TECHNIK","DI  0,75- 8 šedá"]
["TECHNIK","DI  0,75- 8 šedá 100"]
["TECHNIK","DI  0,75-10 bílá"]
["TECHNIK","DI  0,75-10 bílá 100"]
["TECHNIK","DI  0,75-10 modrá"]
["TECHNIK","DI  0,75-10 modrá100"]
["TECHNIK","DI  0,75-10 šedá"]
["TECHNIK","DI  0,75-12 bílá"]
["TECHNIK","DI  0,75-12 bílá 100"]
["TECHNIK","DI  0,75-12 modrá"]
["TECHNIK","DI  0,75-12 šedá"]
["TECHNIK","DI  0,75-18 bílá"]
["TECHNIK","DI  1,0- 6 rudá"]
["TECHNIK","DI  1,0- 6 rudá 100"]
["TECHNIK","DI  1,0- 6 žlutá"]
["TECHNIK","DI  1,0- 6 žlutá 100"]
["TECHNIK","DI  1,0- 8 rudá"]
["TECHNIK","DI  1,0- 8 rudá 100"]
["TECHNIK","DI  1,0- 8 žlutá"]
["TECHNIK","DI  1,0- 8 žlutá 100"]
["TECHNIK","DI  1,0-10 rudá"]
["TECHNIK","DI  1,0-10 rudá 100"]
["TECHNIK","DI  1,0-10 žlutá"]
["TECHNIK","DI  1,0-10 žlutá 100"]
["TECHNIK","DI  1,0-12 rudá"]
["TECHNIK","DI  1,0-12 rudá 100"]
["TECHNIK","DI  1,0-12 žlutá"]
["TECHNIK","DI  1,0-12 žlutá 100"]
["TECHNIK","DI  1,0-18 žlutá"]
["TECHNIK","DI  1,5- 6 černá"]
["TECHNIK","DI  1,5- 6 rudá"]
["TECHNIK","DI  1,5- 6 rudá 100"]
["TECHNIK","DI  1,5- 8 černá"]
["TECHNIK","DI  1,5- 8 černá 100"]
["TECHNIK","DI  1,5- 8 rudá"]
["TECHNIK","DI  1,5- 8 rudá 100"]
["TECHNIK","DI  1,5-10 černá"]
["TECHNIK","DI  1,5-10 černá 100"]
["TECHNIK","DI  1,5-10 rudá"]
["TECHNIK","DI  1,5-10 rudá 100"]
["TECHNIK","DI  1,5-12 černá"]
["TECHNIK","DI  1,5-12 černá 100"]
["TECHNIK","DI  1,5-12 rudá"]
["TECHNIK","DI  1,5-12 rudá 100"]
["TECHNIK","DI  1,5-18 černá"]
["TECHNIK","DI  1,5-18 černá 100"]
["TECHNIK","DI  1,5-18 rudá"]
["TECHNIK","DI  1,5-18 rudá 100"]
["TECHNIK","DI  2,5- 6 modrá"]
["TECHNIK","DI  2,5- 8 modrá"]
["TECHNIK","DI  2,5- 8 modrá 100"]
["TECHNIK","DI  2,5- 8 šedá"]
["TECHNIK","DI  2,5- 8 šedá 100"]
["TECHNIK","DI  2,5-10 modrá"]
["TECHNIK","DI  2,5-10 modrá 100"]
["TECHNIK","DI  2,5-10 šedá"]
["TECHNIK","DI  2,5-12 modrá"]
["TECHNIK","DI  2,5-12 modrá 100"]
["TECHNIK","DI  2,5-12 šedá"]
["TECHNIK","DI  2,5-18 modrá"]
["TECHNIK","DI  2,5-18 modrá 100"]
["TECHNIK","DI  2,5-18 šedá"]
["TECHNIK","DI  2,5-25 modrá"]
["TECHNIK","DI  4-10 oranž 100"]
["TECHNIK","DI  4-10 oranžová"]
["TECHNIK","DI  4-10 šedá"]
["TECHNIK","DI  4-10 šedá 100"]
["TECHNIK","DI  4-12 oranž 100"]
["TECHNIK","DI  4-12 oranžová"]
["TECHNIK","DI  4-12 šedá"]
["TECHNIK","DI  4-12 šedá 100"]
["TECHNIK","DI  4-18 oranžová"]
["TECHNIK","DI  4-18 šedá"]
["TECHNIK","DI  6-12 černá"]
["TECHNIK","DI  6-12 zelená"]
["TECHNIK","DI  6-12 žlutá"]
["TECHNIK","DI  6-18 černá"]
["TECHNIK","DI  6-18 zelená"]
["TECHNIK","DI  6-18 žlutá"]
["TECHNIK","DI 10-12 hnědá"]
["TECHNIK","DI 10-12 rudá"]
["TECHNIK","DI 10-12 sl. kost"]
["TECHNIK","DI 10-18 hnědá"]
["TECHNIK","DI 10-18 rudá"]
["TECHNIK","DI 10-18 sl. kost"]
["TECHNIK","DI 16-12 bílá"]
["TECHNIK","DI 16-12 modrá"]
["TECHNIK","DI 16-12 zelená"]
["TECHNIK","DI 16-18 bílá"]
["TECHNIK","DI 16-18 modrá"]
["TECHNIK","DI 16-18 zelená"]
["TECHNIK","DI 25-16 černá"]
["TECHNIK","DI 25-16 hnědá"]
["TECHNIK","DI 25-16 žlutá"]
["TECHNIK","DI 25-18 hnědá"]
["TECHNIK","DI 25-22 černá"]
["TECHNIK","DI 25-22 hnědá"]
["TECHNIK","DI 25-22 žlutá"]
["TECHNIK","DI 35-16 béžová"]
["TECHNIK","DI 35-16 rudá"]
["TECHNIK","DI 35-18 béžová"]
["TECHNIK","DI 35-25 béžová"]
["TECHNIK","DI 35-25 rudá"]
["TECHNIK","DI 50-20 modrá"]
["TECHNIK","DI 50-20 zelená"]
["TECHNIK","DI 50-25 modrá"]
["TECHNIK","DI 50-25 zelená"]
["TECHNIK","DI 50-30 zelená"]
["TECHNIK","DI 70-20 žlutá"]
["TECHNIK","DI 70-25 žlutá"]
["TECHNIK","DI 95-25 rudá"]
["TECHNIK","DI 95-30 rudá"]
["TECHNIK","DI120-27 modrá"]
["TECHNIK","DI120-34 modrá"]
["TECHNIK","DI150-32 žlutá"]
["TECHNIK","DIF  2,5- 8 modrá"]
["TECHNIK","DIF  2,5-12 modrá"]
["TECHNIK","DIF  4-10 šedá"]
["TECHNIK","DIF 16-12 modrá"]
["TECHNIK","DIZ  1,5- 8 černá"]
["TECHNIK","DIZ  1,5-10 černá"]
["TECHNIK","DIZ  2,5- 8 modrá"]
["TECHNIK","DIZ  2,5-12 modrá"]
["TECHNIK","DIZ  4-10 šedá"]
["TECHNIK","DIZ  6-12 černá"]
["TECHNIK","DIZ 10-12 rudá"]
["TECHNIK","DIZ 16-12 modrá"]
["TECHNIK","DK 11208"]
["TECHNIK","DK 11241"]
["TECHNIK","DK 22212"]
["TECHNIK","DK 22606"]
["TECHNIK","DMT-SET"]
["TECHNIK","DN  0,14- 7"]
["TECHNIK","DN  0,14- 7 / 100"]
["TECHNIK","DN  0,25- 5"]
["TECHNIK","DN  0,25- 5 / 100"]
["TECHNIK","DN  0,25- 7"]
["TECHNIK","DN  0,25- 7 / 100"]
["TECHNIK","DN  0,34- 5"]
["TECHNIK","DN  0,34- 5 / 100"]
["TECHNIK","DN  0,34- 7"]
["TECHNIK","DN  0,34- 7 / 100"]
["TECHNIK","DN  0,5- 6"]
["TECHNIK","DN  0,5- 6 / 100"]
["TECHNIK","DN  0,5- 8"]
["TECHNIK","DN  0,5- 8 / 100"]
["TECHNIK","DN  0,5-10"]
["TECHNIK","DN  0,5-10 / 100"]
["TECHNIK","DN  0,5-12"]
["TECHNIK","DN  0,5-12 / 100"]
["TECHNIK","DN  0,75- 6"]
["TECHNIK","DN  0,75- 6 / 100"]
["TECHNIK","DN  0,75- 8"]
["TECHNIK","DN  0,75- 8 / 100"]
["TECHNIK","DN  0,75-10"]
["TECHNIK","DN  0,75-10 / 100"]
["TECHNIK","DN  0,75-12"]
["TECHNIK","DN  0,75-15"]
["TECHNIK","DN  0,75-15 / 100"]
["TECHNIK","DN  0,75-20"]
["TECHNIK","DN  1,0- 6"]
["TECHNIK","DN  1,0- 6 / 100"]
["TECHNIK","DN  1,0- 8"]
["TECHNIK","DN  1,0- 8 / 100"]
["TECHNIK","DN  1,0-10"]
["TECHNIK","DN  1,0-10 / 100"]
["TECHNIK","DN  1,0-12"]
["TECHNIK","DN  1,0-12 / 100"]
["TECHNIK","DN  1,0-15"]
["TECHNIK","DN  1,0-15 / 100"]
["TECHNIK","DN  1,0-18"]
["TECHNIK","DN  1,0-20"]
["TECHNIK","DN  1,5- 6"]
["TECHNIK","DN  1,5- 6 / 100"]
["TECHNIK","DN  1,5- 7"]
["TECHNIK","DN  1,5- 8"]
["TECHNIK","DN  1,5- 8 / 100"]
["TECHNIK","DN  1,5-10"]
["TECHNIK","DN  1,5-10 / 100"]
["TECHNIK","DN  1,5-12"]
["TECHNIK","DN  1,5-12 / 100"]
["TECHNIK","DN  1,5-15"]
["TECHNIK","DN  1,5-15 / 100"]
["TECHNIK","DN  1,5-18"]
["TECHNIK","DN  1,5-20"]
["TECHNIK","DN  2,5- 7"]
["TECHNIK","DN  2,5- 7 / 100"]
["TECHNIK","DN  2,5- 8"]
["TECHNIK","DN  2,5- 8 / 100"]
["TECHNIK","DN  2,5-10"]
["TECHNIK","DN  2,5-10 / 100"]
["TECHNIK","DN  2,5-12"]
["TECHNIK","DN  2,5-12 / 100"]
["TECHNIK","DN  2,5-15"]
["TECHNIK","DN  2,5-18"]
["TECHNIK","DN  2,5-18 / 100"]
["TECHNIK","DN  2,5-20"]
["TECHNIK","DN  2,5-25"]
["TECHNIK","DN  4- 9"]
["TECHNIK","DN  4- 9 / 100"]
["TECHNIK","DN  4-10"]
["TECHNIK","DN  4-10 / 100"]
["TECHNIK","DN  4-12"]
["TECHNIK","DN  4-12 / 100"]
["TECHNIK","DN  4-15"]
["TECHNIK","DN  4-18"]
["TECHNIK","DN  4-18 / 100"]
["TECHNIK","DN  4-20"]
["TECHNIK","DN  6- 6"]
["TECHNIK","DN  6-10"]
["TECHNIK","DN  6-10 / 100"]
["TECHNIK","DN  6-12"]
["TECHNIK","DN  6-12 / 100"]
["TECHNIK","DN  6-15"]
["TECHNIK","DN  6-18"]
["TECHNIK","DN  6-18 / 100"]
["TECHNIK","DN  6-20"]
["TECHNIK","DN 10-12"]
["TECHNIK","DN 10-12 / 100"]
["TECHNIK","DN 10-15"]
["TECHNIK","DN 10-18"]
["TECHNIK","DN 10-20"]
["TECHNIK","DN 10-25"]
["TECHNIK","DN 16-12"]
["TECHNIK","DN 16-15"]
["TECHNIK","DN 16-18"]
["TECHNIK","DN 16-20"]
["TECHNIK","DN 16-25"]
["TECHNIK","DN 16-32"]
["TECHNIK","DN 25-12"]
["TECHNIK","DN 25-15"]
["TECHNIK","DN 25-18"]
["TECHNIK","DN 25-25"]
["TECHNIK","DN 25-32"]
["TECHNIK","DN 35-12"]
["TECHNIK","DN 35-15"]
["TECHNIK","DN 35-18"]
["TECHNIK","DN 35-20"]
["TECHNIK","DN 35-25"]
["TECHNIK","DN 35-32"]
["TECHNIK","DN 50-12"]
["TECHNIK","DN 50-18"]
["TECHNIK","DN 50-22"]
["TECHNIK","DN 50-25"]
["TECHNIK","DN 50-32"]
["TECHNIK","DN 70-25"]
["TECHNIK","DN 70-32"]
["TECHNIK","DN 95-25"]
["TECHNIK","DN 95-32"]
["TECHNIK","DN120-32"]
["TECHNIK","DN120-38"]
["TECHNIK","DN150-32"]
["TECHNIK","DN150-38"]
["TECHNIK","DN185-32"]
["TECHNIK","DN185-40"]
["TECHNIK","DN240-40"]
["TECHNIK","DP 0,5- 8 bílá"]
["TECHNIK","DP 0,5- 8 oranžová"]
["TECHNIK","DP 0,75- 8 bílá"]
["TECHNIK","DP 0,75- 8 šedá"]
["TECHNIK","DP 0,75-8 modrá"]
["TECHNIK","DP 1,0- 8 rudá"]
["TECHNIK","DP 1,0- 8 žlutá"]
["TECHNIK","DP 1,5- 8 černá"]
["TECHNIK","DP 1,5- 8 rudá"]
["TECHNIK","DP 2,5- 8 modrá"]
["TECHNIK","DP 2,5- 8 šedá"]
["TECHNIK SPECIAL - AKCIA","DP100Z PLUS"]
["TECHNIK SPECIAL - AKCIA","DR 30"]
["TECHNIK SPECIAL - AKCIA","DR 50"]
["TECHNIK","DRMC 0,25-8 modrá"]
["TECHNIK","DRMC 0,34-8 tyrkys"]
["TECHNIK","DRMC 0,5-8 bílá"]
["TECHNIK","DRMC 0,5-8 oranžová"]
["TECHNIK","DRMC 0,75-8 bílá"]
["TECHNIK","DRMC 0,75-8 šedá"]
["TECHNIK","DRMC 1,0-8 rudá"]
["TECHNIK","DRMC 1,0-8 žlutá"]
["TECHNIK","DRMC 1,5-8 černá"]
["TECHNIK","DRMC 1,5-8 rudá"]
["TECHNIK","DRMC 2,5-8 modrá"]
["TECHNIK SPECIAL - AKCIA","DRN 400"]
["TECHNIK SPECIAL - AKCIA","DRO 500"]
["TECHNIK","DRS 0,34-8 tyrkysová"]
["TECHNIK","DRS 0,5-8 bílá"]
["TECHNIK","DRS 0,5-8 oranžová"]
["TECHNIK","DRS 0,75-8 bílá"]
["TECHNIK","DRS 0,75-8 modrá"]
["TECHNIK","DRS 0,75-8 šedá"]
["TECHNIK","DRS 1,0-8 rudá"]
["TECHNIK","DRS 1,0-8 žlutá"]
["TECHNIK","DRS 1,5-8 černá"]
["TECHNIK","DRS 1,5-8 rudá"]
["TECHNIK","DRS 2,5-8 modrá"]
["TECHNIK","DRS 2,5-8 šedá"]
["TECHNIK SPECIAL - AKCIA","DRT  9,0"]
["TECHNIK SPECIAL - AKCIA","DRT 11,0"]
["TECHNIK SPECIAL - AKCIA","DRT 13,0"]
["TECHNIK SPECIAL - AKCIA","DRT 18,0"]
["TECHNIK SPECIAL - AKCIA","DRT 22x13"]
["TECHNIK SPECIAL - AKCIA","DSP 120"]
["TECHNIK SPECIAL - AKCIA","DSP 120 nožní ovl.  "]
["TECHNIK SPECIAL - AKCIA","DUO"]
["TECHNIK","DUSPOL analog"]
["TECHNIK","DUSPOL combi"]
["TECHNIK","DUSPOL digital"]
["TECHNIK","DUSPOL expert"]
["TECHNIK","DUSPOL master"]
["TECHNIK","DUTEST PRO"]
["TECHNIK","DYMO 1540"]
["TECHNIK","DYMO adaptér 9V"]
["TECHNIK","DYMO adaptér12V"]
["TECHNIK","DYMO baterie"]
["TECHNIK","DYMO Junior"]
["TECHNIK","DYMO M11"]
["TECHNIK","DYMO Omega"]
["TECHNIK SPECIAL - AKCIA","EC 65"]
["TECHNIK SPECIAL - AKCIA","EC PP"]
["TECHNIK SPECIAL - AKCIA","EC PP OI056"]
["TECHNIK SPECIAL - AKCIA","EC PP SK0144"]
["TECHNIK SPECIAL - AKCIA","ECM 03-N"]
["TECHNIK","ECOSTRIP 6"]
["TECHNIK SPECIAL - AKCIA","ECW-H3D"]
["TECHNIK","EDDING 140 S černá"]
["TECHNIK","EDDING 140 S modrá"]
["TECHNIK","EDDING 140 S oranž."]
["TECHNIK","EDDING 140 S rudá"]
["TECHNIK","EDDING 140 S žlutá"]
["TECHNIK","EDDING 141 F černá"]
["TECHNIK","EDDING 141 F modrá"]
["TECHNIK","EDDING 141 F oranž"]
["TECHNIK","EDDING 141 F rudá"]
["TECHNIK","EDDING 141 F zelená"]
["TECHNIK","EDDING 141 F žlutá"]
["TECHNIK","EDDING 142 M černá"]
["TECHNIK","EDDING 142 M fialová"]
["TECHNIK","EDDING 142 M modrá"]
["TECHNIK","EDDING 142 M oranž"]
["TECHNIK","EDDING 142 M rudá"]
["TECHNIK","EDDING 142 M žlutá"]
["TECHNIK","EDDING 143 B černá"]
["TECHNIK","EDDING 143 B rudá"]
["TECHNIK","EDDING 147 S černá"]
["TECHNIK","EDDING 147 S modrá"]
["TECHNIK","EDDING 147 S rudá"]
["TECHNIK","EDDING 147 S zelená"]
["TECHNIK","EDDING 149 M černá"]
["TECHNIK","EDDING 149 M modrá"]
["TECHNIK","EDDING 149 M rudá"]
["TECHNIK","EDDING 149 M zelená"]
["TECHNIK","EDDING 404 černá"]
["TECHNIK","EDDING 750 bílá"]
["TECHNIK","EDDING 750 černá"]
["TECHNIK","EDDING 750 fialová"]
["TECHNIK","EDDING 750 modrá"]
["TECHNIK","EDDING 750 rudá"]
["TECHNIK","EDDING 750 zelená"]
["TECHNIK","EDDING 750 žlutá"]
["TECHNIK","EDDING 751 bílá"]
["TECHNIK","EDDING 751 černá"]
["TECHNIK","EDDING 780 bílá"]
["TECHNIK","EDDING 790 bílá"]
["TECHNIK","EDDING 790 černá"]
["TECHNIK","EDDING 790 modrá"]
["TECHNIK","EDDING 790 rudá"]
["TECHNIK","EDDING 790 stříbrná"]
["TECHNIK","EDDING 790 zelená"]
["TECHNIK","EDDING 790 zlatá"]
["TECHNIK","EDDING 790 žlutá"]
["TECHNIK","EDDING 791 bílá"]
["TECHNIK","EDDING 791 černá"]
["TECHNIK","EDDING 791 modrá"]
["TECHNIK","EDDING 791 rudá"]
["TECHNIK","EDDING 791 stříbrná"]
["TECHNIK","EDDING 791 zelená"]
["TECHNIK","EDDING 791 zlatá"]
["TECHNIK","EDDING 791 žlutá"]
["TECHNIK","EDDING 792 bílá"]
["TECHNIK","EDDING 792 černá"]
["TECHNIK","EDDING 792 modrá"]
["TECHNIK","EDDING 792 rudá"]
["TECHNIK","EDDING 792 stříbrná"]
["TECHNIK","EDDING 792 zelená"]
["TECHNIK","EDDING 792 zlatá"]
["TECHNIK","EDDING 8200 šedá"]
["TECHNIK","EDDING 8300 černá"]
["TECHNIK","EDDING 8400 černá"]
["TECHNIK","EDDING 8400 modrá"]
["TECHNIK","EDDING 8407 mix"]
["TECHNIK","EDDING 8500 RW"]
["TECHNIK","EDDING 8750 bílá"]
["TECHNIK","EDDING 8750 černá"]
["TECHNIK","EDDING 8750 modrá"]
["TECHNIK","EDDING 8750 rudá"]
["TECHNIK","EDDING 8750 zelená"]
["TECHNIK","EDDING 8750 žlutá"]
["TECHNIK","EDDING 8850 černá"]
["TECHNIK","EDH 265"]
["TECHNIK SPECIAL - AKCIA","EHP 1"]
["REIKU-B","EMV M16"]
["REIKU-B","EMV M20"]
["REIKU-B","EMV M25"]
["REIKU-B","EMV M32"]
["REIKU-B","EMV M40"]
["REIKU-B","EMV M50"]
["REIKU-B","EMV M63"]
["REIKU-B","EMV P16"]
["REIKU-B","EMV P21"]
["REIKU-B","EMV P29"]
["REIKU-B","EMV P36"]
["REIKU-B","EMV P48"]
["TECHNIK","EP 15x10 bílá"]
["TECHNIK","EP 15x10 color"]
["TECHNIK","EP 15x10 černá"]
["TECHNIK","EP 15x10 fialová"]
["TECHNIK","EP 15x10 hnědá"]
["TECHNIK","EP 15x10 rudá"]
["TECHNIK","EP 15x10 sv.modrá"]
["TECHNIK","EP 15x10 šedá"]
["TECHNIK","EP 15x10 tm.modrá"]
["TECHNIK","EP 15x10 zelená"]
["TECHNIK","EP 15x10 žlutá"]
["TECHNIK","EP 15x10 žz"]
["TECHNIK","EP 15x20.SF bílá"]
["TECHNIK","EP 15x20.SF černá"]
["TECHNIK","EP 15x20.SF fialová"]
["TECHNIK","EP 15x20.SF hnědá"]
["TECHNIK","EP 15x20.SF modrá"]
["TECHNIK","EP 15x20.SF rudá"]
["TECHNIK","EP 15x20.SF šedá"]
["TECHNIK","EP 15x20.SF zelená"]
["TECHNIK","EP 15x20.SF žlutá"]
["TECHNIK","EP 19x18 MV černá"]
["TECHNIK","EP 19x20 bílá"]
["TECHNIK","EP 19x20 color"]
["TECHNIK","EP 19x20 černá"]
["TECHNIK","EP 19x20 modrá"]
["TECHNIK","EP 19x20 rudá"]
["TECHNIK","EP 19x20 šedá"]
["TECHNIK","EP 19x20 zelená"]
["TECHNIK","EP 19x20 žlutá"]
["TECHNIK","EP 19x20 žz"]
["TECHNIK","EP 19x20.SF bílá"]
["TECHNIK","EP 19x20.SF černá"]
["TECHNIK","EP 19x20.SF modrá"]
["TECHNIK","EP 19x20.SF rudá"]
["TECHNIK","EP 19x20.SF zelená"]
["TECHNIK","EP 19x20.SF žlutá"]
["TECHNIK","EP 25x18 MV černá"]
["TECHNIK","EP 25x20 černá"]
["TECHNIK","EP 25x20 žz"]
["TECHNIK","EP 25x20.SF bílá"]
["TECHNIK","EP 25x20.SF černá"]
["TECHNIK","EP 25x20.SF modrá"]
["TECHNIK","EP 25x20.SF rudá"]
["TECHNIK","EP 38x20 černá"]
["TECHNIK","EP 38x20.SF černá"]
["TECHNIK","EP 45x 5 HELP"]
["TECHNIK","EP 50x10 černá"]
["TECHNIK","EP 50x20 černá"]
["TECHNIK","EP 50x20.SF bílá"]
["TECHNIK","EP 50x20.SF černá"]
["TECHNIK","EP 50x20.SF modrá"]
["TECHNIK","EP 701-40/50x10"]
["TECHNIK","EP3M 15x10 černá"]
["TECHNIK","EP3M 15x10 modrá"]
["TECHNIK","EP3M 15x10 rudá"]
["TECHNIK","EP3M 15x10 zelená"]
["TECHNIK","EP3M 15x10 žz"]
["TECHNIK","EP3M 19x20 černá"]
["TECHNIK","EP3M 19x20 rudá"]
["TECHNIK","EP3M 19x33 typ 69"]
["TECHNIK","EP3M 19x9,1 černá"]
["TECHNIK","EP3M 25x7 černá"]
["TECHNIK","EP3M 25x9,1 černá"]
["TECHNIK","EP3M 38x33 černá"]
["TECHNIK","EPAL 50x50"]
["TECHNIK SPECIAL - AKCIA","EP-D 0141"]
["TECHNIK SPECIAL - AKCIA","EP-D 0525"]
["TECHNIK SPECIAL - AKCIA","EPG 10"]
["TECHNIK SPECIAL - AKCIA","EPG 15"]
["TECHNIK SPECIAL - AKCIA","EPG 20"]
["TECHNIK SPECIAL - AKCIA","EP-MAG"]
["TECHNIK","EPT 25x9 šedá"]
["TECHNIK","EPV  50x33 žl-černá"]
["TECHNIK","FC 0605"]
["TECHNIK","FLEXI-CRIMP 6"]
["TECHNIK","FLUKE 2042"]
["TECHNIK","FLUKE T110"]
["TECHNIK","FLUKE T130"]
["TECHNIK","FLUKE T150"]
["TECHNIK SPECIAL - AKCIA","FP 700"]
["TECHNIK SPECIAL - AKCIA","FP 850"]
["TECHNIK SPECIAL - AKCIA","FP brašna"]
["TECHNIK SPECIAL - AKCIA","FPA 700"]
["REIKU-B","FSMF-29-600"]
["REIKU-B","FSMF-36-400"]
["REIKU-B","FSMF-36-600"]
["REIKU-B","FSMF-48-550"]
["REIKU-B","FSMF-52-1000"]
["REIKU-B","FSMF-52-52-1000"]
["REIKU-B","FSMF-70-1000"]
["REIKU-B","FSMF-70-550"]
["REIKU-B","FSSF-23-600"]
["REIKU-B","FSSF-29-400"]
["REIKU-B","FSSF-36-400"]
["REIKU-B","FSVF-52-1000"]
["REIKU-B","FSVF-70-1000"]
["TECHNIK","GH-29"]
["TECHNIK SPECIAL - AKCIA","GRAFITOVÁ PASTA"]
["TECHNIK SPECIAL - AKCIA","HAD 2"]
["TECHNIK SPECIAL - AKCIA","HAD 3"]
["TECHNIK SPECIAL - AKCIA","HAD 5"]
["TECHNIK SPECIAL - AKCIA","HAD10"]
["TECHNIK SPECIAL - AKCIA","HC 20"]
["TECHNIK SPECIAL - AKCIA","HC 20/ 6 STD"]
["TECHNIK","HF 0525"]
["TECHNIK","HF 1"]
["TECHNIK","HF 1 crimpstar"]
["TECHNIK","HF 1/TF"]
["TECHNIK","HF 2"]
["TECHNIK","HF 2/Z"]
["TECHNIK","HF 2/Z/LOC"]
["TECHNIK","HF 3"]
["TECHNIK","HF-BP"]
["TECHNIK SPECIAL - AKCIA","HK 60 22"]
["TECHNIK","Hledač netěsností"]
["TECHNIK","Hliníkový sprej"]
["TECHNIK","HN 1"]
["TECHNIK","HN 1 crimpstar"]
["TECHNIK","HN 1/TF"]
["TECHNIK","HN 1/Y"]
["TECHNIK","HN 2"]
["TECHNIK","HN 35"]
["TECHNIK","HN 5 crimpstar"]
["TECHNIK","HN 5/Y"]
["TECHNIK","HN 7"]
["TECHNIK","HN 7/TF"]
["TECHNIK","HNKE  4"]
["TECHNIK","HNKE  4/TF"]
["TECHNIK","HNKE  6"]
["TECHNIK","HNKE  6/TF"]
["TECHNIK","HNKE  616"]
["TECHNIK","HNKE  6U6"]
["TECHNIK","HNKE 02516"]
["TECHNIK","HNKE 02516/TF"]
["TECHNIK","HNKE 10P"]
["TECHNIK","HNKE 10U6"]
["TECHNIK","HNKE 16"]
["TECHNIK","HNKE 16/TF"]
["TECHNIK","HNKE 1635"]
["TECHNIK","HNKE 16P"]
["TECHNIK","HNKE 16U"]
["TECHNIK","HNKE 25/50"]
["TECHNIK","HNKE 25/50/TF"]
["TECHNIK","HNKE 35"]
["TECHNIK","HNKE 35/TF"]
["TECHNIK","HNKE 50 crimpstar"]
["TECHNIK","HNKE 50L"]
["TECHNIK","HNKE 50L/TF"]
["TECHNIK","HNN 3"]
["TECHNIK","HNN 4"]
["TECHNIK","HP 1 crimpstar"]
["TECHNIK","HP 1/Z"]
["TECHNIK","HP 2/Z"]
["TECHNIK","HP 3"]
["TECHNIK","HP 3 crimpstar"]
["TECHNIK","HP 3/TF"]
["TECHNIK","HP 3/Y"]
["TECHNIK SPECIAL - AKCIA","HP 60 CK"]
["TECHNIK","HP4-C10"]
["TECHNIK","HPH 1 crimpstar"]
["TECHNIK","HSe 211"]
["TECHNIK","HSe 221"]
["TECHNIK","HSe 231"]
["TECHNIK","HSe 241"]
["TECHNIK","HSe 251"]
["TECHNIK SPECIAL - AKCIA","HT 131-C"]
["TECHNIK SPECIAL - AKCIA","HT 131LN-C"]
["TECHNIK SPECIAL - AKCIA","HT 131-UC"]
["TECHNIK SPECIAL - AKCIA","HT 45E"]
["TECHNIK SPECIAL - AKCIA","HT 51"]
["TECHNIK","HTI  1,2 bílá"]
["TECHNIK","HTI  1,2 bílá R"]
["TECHNIK","HTI  1,2 černá"]
["TECHNIK","HTI  1,2 černá R"]
["TECHNIK","HTI  1,2 modrá"]
["TECHNIK","HTI  1,2 modrá R"]
["TECHNIK","HTI  1,2 rudá"]
["TECHNIK","HTI  1,2 rudá R"]
["TECHNIK","HTI  1,2 transp"]
["TECHNIK","HTI  1,2 transp R"]
["TECHNIK","HTI  1,2 žlutá"]
["TECHNIK","HTI  1,2 žlutá R"]
["TECHNIK","HTI  1,6 bílá"]
["TECHNIK","HTI  1,6 bílá R"]
["TECHNIK","HTI  1,6 černá"]
["TECHNIK","HTI  1,6 černá R"]
["TECHNIK","HTI  1,6 modrá"]
["TECHNIK","HTI  1,6 modrá R"]
["TECHNIK","HTI  1,6 rudá"]
["TECHNIK","HTI  1,6 rudá R"]
["TECHNIK","HTI  1,6 šedá"]
["TECHNIK","HTI  1,6 šedá R"]
["TECHNIK","HTI  1,6 transp"]
["TECHNIK","HTI  1,6 transp R"]
["TECHNIK","HTI  1,6 žlutá"]
["TECHNIK","HTI  1,6 žlutá R"]
["TECHNIK","HTI  1,6 žz"]
["TECHNIK","HTI  1,6 žz R"]
["TECHNIK","HTI  2,4 bílá"]
["TECHNIK","HTI  2,4 bílá R"]
["TECHNIK","HTI  2,4 bílá T2"]
["TECHNIK","HTI  2,4 bílá T3"]
["TECHNIK","HTI  2,4 černá"]
["TECHNIK","HTI  2,4 černá R"]
["TECHNIK","HTI  2,4 hnědá"]
["TECHNIK","HTI  2,4 hnědá R"]
["TECHNIK","HTI  2,4 modrá"]
["TECHNIK","HTI  2,4 modrá R"]
["TECHNIK","HTI  2,4 oranžová"]
["TECHNIK","HTI  2,4 oranžová R"]
["TECHNIK","HTI  2,4 rudá"]
["TECHNIK","HTI  2,4 rudá R"]
["TECHNIK","HTI  2,4 šedá"]
["TECHNIK","HTI  2,4 šedá R"]
["TECHNIK","HTI  2,4 transp"]
["TECHNIK","HTI  2,4 transp R"]
["TECHNIK","HTI  2,4 zelená"]
["TECHNIK","HTI  2,4 zelená R"]
["TECHNIK","HTI  2,4 žlutá"]
["TECHNIK","HTI  2,4 žlutá R"]
["TECHNIK","HTI  2,4 žlutá T2"]
["TECHNIK","HTI  2,4 žlutá T3"]
["TECHNIK","HTI  2,4 žz"]
["TECHNIK","HTI  2,4 žz R"]
["TECHNIK","HTI  3,2 bílá"]
["TECHNIK","HTI  3,2 bílá R"]
["TECHNIK","HTI  3,2 bílá T1"]
["TECHNIK","HTI  3,2 bílá T2"]
["TECHNIK","HTI  3,2 bílá T3"]
["TECHNIK","HTI  3,2 černá"]
["TECHNIK","HTI  3,2 černá R"]
["TECHNIK","HTI  3,2 hnědá"]
["TECHNIK","HTI  3,2 hnědá R"]
["TECHNIK","HTI  3,2 modrá"]
["TECHNIK","HTI  3,2 modrá R"]
["TECHNIK","HTI  3,2 oranžová"]
["TECHNIK","HTI  3,2 oranžová R"]
["TECHNIK","HTI  3,2 rudá"]
["TECHNIK","HTI  3,2 rudá R"]
["TECHNIK","HTI  3,2 šedá"]
["TECHNIK","HTI  3,2 šedá R"]
["TECHNIK","HTI  3,2 transp"]
["TECHNIK","HTI  3,2 transp R"]
["TECHNIK","HTI  3,2 zelená"]
["TECHNIK","HTI  3,2 zelená R"]
["TECHNIK","HTI  3,2 žlutá"]
["TECHNIK","HTI  3,2 žlutá R"]
["TECHNIK","HTI  3,2 žlutá T1"]
["TECHNIK","HTI  3,2 žlutá T2"]
["TECHNIK","HTI  3,2 žlutá T3"]
["TECHNIK","HTI  3,2 žz"]
["TECHNIK","HTI  3,2 žz R"]
["TECHNIK","HTI  4,0 černá"]
["TECHNIK","HTI  4,0 černá R"]
["TECHNIK","HTI  4,8 bílá"]
["TECHNIK","HTI  4,8 bílá R"]
["TECHNIK","HTI  4,8 bílá T1"]
["TECHNIK","HTI  4,8 bílá T3"]
["TECHNIK","HTI  4,8 černá"]
["TECHNIK","HTI  4,8 černá R"]
["TECHNIK","HTI  4,8 fialová"]
["TECHNIK","HTI  4,8 fialová R"]
["TECHNIK","HTI  4,8 hnědá"]
["TECHNIK","HTI  4,8 hnědá R"]
["TECHNIK","HTI  4,8 modrá"]
["TECHNIK","HTI  4,8 modrá R"]
["TECHNIK","HTI  4,8 oranžová R"]
["TECHNIK","HTI  4,8 rudá"]
["TECHNIK","HTI  4,8 rudá R"]
["TECHNIK","HTI  4,8 šedá"]
["TECHNIK","HTI  4,8 šedá R"]
["TECHNIK","HTI  4,8 transp"]
["TECHNIK","HTI  4,8 transp R"]
["TECHNIK","HTI  4,8 zelená"]
["TECHNIK","HTI  4,8 zelená R"]
["TECHNIK","HTI  4,8 žlutá"]
["TECHNIK","HTI  4,8 žlutá R"]
["TECHNIK","HTI  4,8 žlutá T1"]
["TECHNIK","HTI  4,8 žlutá T3"]
["TECHNIK","HTI  4,8 žz"]
["TECHNIK","HTI  4,8 žz R"]
["TECHNIK","HTI  6,4 bílá"]
["TECHNIK","HTI  6,4 bílá R"]
["TECHNIK","HTI  6,4 bílá T1"]
["TECHNIK","HTI  6,4 bílá T3"]
["TECHNIK","HTI  6,4 černá"]
["TECHNIK","HTI  6,4 černá R"]
["TECHNIK","HTI  6,4 hnědá"]
["TECHNIK","HTI  6,4 hnědá R"]
["TECHNIK","HTI  6,4 modrá"]
["TECHNIK","HTI  6,4 modrá R"]
["TECHNIK","HTI  6,4 rudá"]
["TECHNIK","HTI  6,4 rudá R"]
["TECHNIK","HTI  6,4 šedá"]
["TECHNIK","HTI  6,4 šedá R"]
["TECHNIK","HTI  6,4 transp"]
["TECHNIK","HTI  6,4 transp R"]
["TECHNIK","HTI  6,4 zelená"]
["TECHNIK","HTI  6,4 zelená R"]
["TECHNIK","HTI  6,4 žlutá"]
["TECHNIK","HTI  6,4 žlutá R"]
["TECHNIK","HTI  6,4 žlutá T1"]
["TECHNIK","HTI  6,4 žlutá T3"]
["TECHNIK","HTI  6,4 žz"]
["TECHNIK","HTI  6,4 žz R"]
["TECHNIK","HTI  7,0 černá R"]
["TECHNIK","HTI  8,0 černá"]
["TECHNIK","HTI  8,0 černá R"]
["TECHNIK","HTI  9,5 bílá"]
["TECHNIK","HTI  9,5 bílá R"]
["TECHNIK","HTI  9,5 bílá T3"]
["TECHNIK","HTI  9,5 černá"]
["TECHNIK","HTI  9,5 černá R"]
["TECHNIK","HTI  9,5 modrá"]
["TECHNIK","HTI  9,5 modrá R"]
["TECHNIK","HTI  9,5 oranž R"]
["TECHNIK","HTI  9,5 rudá"]
["TECHNIK","HTI  9,5 rudá R"]
["TECHNIK","HTI  9,5 šedá"]
["TECHNIK","HTI  9,5 šedá R"]
["TECHNIK","HTI  9,5 transp"]
["TECHNIK","HTI  9,5 transp R"]
["TECHNIK","HTI  9,5 zelená"]
["TECHNIK","HTI  9,5 zelená R"]
["TECHNIK","HTI  9,5 žlutá"]
["TECHNIK","HTI  9,5 žlutá R"]
["TECHNIK","HTI  9,5 žlutá T3"]
["TECHNIK","HTI  9,5 žz"]
["TECHNIK","HTI  9,5 žz R"]
["TECHNIK","HTI 12,0 černá R"]
["TECHNIK","HTI 12,7 bílá"]
["TECHNIK","HTI 12,7 bílá R"]
["TECHNIK","HTI 12,7 černá"]
["TECHNIK","HTI 12,7 černá R"]
["TECHNIK","HTI 12,7 modrá"]
["TECHNIK","HTI 12,7 modrá R"]
["TECHNIK","HTI 12,7 oranž R"]
["TECHNIK","HTI 12,7 oranžová"]
["TECHNIK","HTI 12,7 rudá"]
["TECHNIK","HTI 12,7 rudá R"]
["TECHNIK","HTI 12,7 šedá"]
["TECHNIK","HTI 12,7 šedá R"]
["TECHNIK","HTI 12,7 transp"]
["TECHNIK","HTI 12,7 transp R"]
["TECHNIK","HTI 12,7 zelená R"]
["TECHNIK","HTI 12,7 žlutá"]
["TECHNIK","HTI 12,7 žlutá R"]
["TECHNIK","HTI 12,7 žz"]
["TECHNIK","HTI 12,7 žz R"]
["TECHNIK","HTI 16,0 černá"]
["TECHNIK","HTI 16,0 černá R"]
["TECHNIK","HTI 16,0 modrá R"]
["TECHNIK","HTI 16,0 transp R"]
["TECHNIK","HTI 16,0 žlutá R"]
["TECHNIK","HTI 19,0 bílá"]
["TECHNIK","HTI 19,0 bílá R"]
["TECHNIK","HTI 19,0 bílá RW"]
["TECHNIK","HTI 19,0 černá"]
["TECHNIK","HTI 19,0 černá R"]
["TECHNIK","HTI 19,0 modrá"]
["TECHNIK","HTI 19,0 modrá R"]
["TECHNIK","HTI 19,0 rudá"]
["TECHNIK","HTI 19,0 rudá R"]
["TECHNIK","HTI 19,0 šedá"]
["TECHNIK","HTI 19,0 šedá R"]
["TECHNIK","HTI 19,0 transp"]
["TECHNIK","HTI 19,0 transp R"]
["TECHNIK","HTI 19,0 žlutá"]
["TECHNIK","HTI 19,0 žlutá R"]
["TECHNIK","HTI 19,0 žz"]
["TECHNIK","HTI 19,0 žz R"]
["TECHNIK","HTI 25,4 bílá"]
["TECHNIK","HTI 25,4 bílá R"]
["TECHNIK","HTI 25,4 bílá RW"]
["TECHNIK","HTI 25,4 černá"]
["TECHNIK","HTI 25,4 černá R"]
["TECHNIK","HTI 25,4 modrá"]
["TECHNIK","HTI 25,4 modrá R"]
["TECHNIK","HTI 25,4 oranž R"]
["TECHNIK","HTI 25,4 rudá"]
["TECHNIK","HTI 25,4 rudá R"]
["TECHNIK","HTI 25,4 šedá"]
["TECHNIK","HTI 25,4 šedá R"]
["TECHNIK","HTI 25,4 transp"]
["TECHNIK","HTI 25,4 transp R"]
["TECHNIK","HTI 25,4 žlutá"]
["TECHNIK","HTI 25,4 žlutá R"]
["TECHNIK","HTI 25,4 žz"]
["TECHNIK","HTI 25,4 žz R"]
["TECHNIK","HTI 30,0 černá"]
["TECHNIK","HTI 30,0 černá R"]
["TECHNIK","HTI 38,0 bílá"]
["TECHNIK","HTI 38,0 bílá R"]
["TECHNIK","HTI 38,0 černá"]
["TECHNIK","HTI 38,0 černá R"]
["TECHNIK","HTI 38,0 modrá"]
["TECHNIK","HTI 38,0 modrá R"]
["TECHNIK","HTI 38,0 oranž"]
["TECHNIK","HTI 38,0 oranž R"]
["TECHNIK","HTI 38,0 rudá"]
["TECHNIK","HTI 38,0 rudá R"]
["TECHNIK","HTI 38,0 šedá"]
["TECHNIK","HTI 38,0 šedá R"]
["TECHNIK","HTI 38,0 transp"]
["TECHNIK","HTI 38,0 transp R"]
["TECHNIK","HTI 38,0 žlutá"]
["TECHNIK","HTI 38,0 žlutá R"]
["TECHNIK","HTI 38,0 žz"]
["TECHNIK","HTI 38,0 žz R"]
["TECHNIK","HTI 51,0 bílá"]
["TECHNIK","HTI 51,0 bílá R"]
["TECHNIK","HTI 51,0 černá"]
["TECHNIK","HTI 51,0 černá R"]
["TECHNIK","HTI 51,0 modrá"]
["TECHNIK","HTI 51,0 modrá R"]
["TECHNIK","HTI 51,0 oranž R"]
["TECHNIK","HTI 51,0 oranžová"]
["TECHNIK","HTI 51,0 rudá"]
["TECHNIK","HTI 51,0 rudá R"]
["TECHNIK","HTI 51,0 šedá"]
["TECHNIK","HTI 51,0 šedá R"]
["TECHNIK","HTI 51,0 transp"]
["TECHNIK","HTI 51,0 transp R"]
["TECHNIK","HTI 51,0 zelená"]
["TECHNIK","HTI 51,0 zelená R"]
["TECHNIK","HTI 51,0 žz"]
["TECHNIK","HTI 51,0 žz R"]
["TECHNIK","HTI 76,2 bílá R"]
["TECHNIK","HTI 76,2 černá"]
["TECHNIK","HTI 76,2 černá R"]
["TECHNIK","HTI 76,2 modrá R"]
["TECHNIK","HTI 76,2 rudá"]
["TECHNIK","HTI 76,2 rudá R"]
["TECHNIK","HTI 76,2 šedá"]
["TECHNIK","HTI 76,2 šedá R"]
["TECHNIK","HTI 76,2 transp"]
["TECHNIK","HTI 76,2 transp R"]
["TECHNIK","HTI 76,2 zelená"]
["TECHNIK","HTI 76,2 zelená R"]
["TECHNIK","HTI 76,2 žz"]
["TECHNIK","HTI 76,2 žz R"]
["TECHNIK","HTI102,0 černá"]
["TECHNIK","HTI102,0 černá R"]
["TECHNIK","HTI102,0 modrá"]
["TECHNIK","HTI102,0 modrá R"]
["TECHNIK","HTI102,0 rudá"]
["TECHNIK","HTI102,0 rudá R"]
["TECHNIK","HTI102,0 transp"]
["TECHNIK","HTI102,0 transp R"]
["TECHNIK","HTI126,0 černá"]
["TECHNIK","HTI150,0 černá"]
["TECHNIK","HTI180,0 černá"]
["TECHNIK","HTI200,0 černá"]
["TECHNIK","HTI250,0 černá"]
["TECHNIK","HTI300,0 černá"]
["TECHNIK","HTI350,0 černá"]
["TECHNIK","HTN  1,2/20 bílá"]
["TECHNIK","HTN  1,2/20 černá"]
["TECHNIK","HTN  1,2/20 modrá"]
["TECHNIK","HTN  1,2/20 rudá"]
["TECHNIK","HTN  1,2/20 zelená"]
["TECHNIK","HTN  1,2/20 žlutá"]
["TECHNIK","HTN  1,2/30 černá"]
["TECHNIK","HTN  1,2/30 transp"]
["TECHNIK","HTN  1,6/20 bílá"]
["TECHNIK","HTN  1,6/20 černá"]
["TECHNIK","HTN  1,6/20 modrá"]
["TECHNIK","HTN  1,6/20 rudá"]
["TECHNIK","HTN  1,6/20 zelená"]
["TECHNIK","HTN  1,6/20 žlutá"]
["TECHNIK","HTN  1,6/25 transp"]
["TECHNIK","HTN  1,6/30 bílá"]
["TECHNIK","HTN  1,6/30 černá"]
["TECHNIK","HTN  1,6/30 modrá"]
["TECHNIK","HTN  1,6/30 rudá"]
["TECHNIK","HTN  1,6/30 šedá"]
["TECHNIK","HTN  2,4/15 černá"]
["TECHNIK","HTN  2,4/20 bílá"]
["TECHNIK","HTN  2,4/20 černá"]
["TECHNIK","HTN  2,4/20 modrá"]
["TECHNIK","HTN  2,4/20 rudá"]
["TECHNIK","HTN  2,4/20 zelená"]
["TECHNIK","HTN  2,4/20 žlutá"]
["TECHNIK","HTN  2,4/30 bílá"]
["TECHNIK","HTN  2,4/30 černá"]
["TECHNIK","HTN  2,4/30 hnědá"]
["TECHNIK","HTN  2,4/30 modrá"]
["TECHNIK","HTN  2,4/30 rudá"]
["TECHNIK","HTN  2,4/30 šedá"]
["TECHNIK","HTN  2,4/30 transp"]
["TECHNIK","HTN  2,4/30 žz"]
["TECHNIK","HTN  3,2/20 bílá"]
["TECHNIK","HTN  3,2/20 černá"]
["TECHNIK","HTN  3,2/20 modrá"]
["TECHNIK","HTN  3,2/20 rudá"]
["TECHNIK","HTN  3,2/20 transp"]
["TECHNIK","HTN  3,2/20 zelená"]
["TECHNIK","HTN  3,2/20 žlutá"]
["TECHNIK","HTN  3,2/30 bílá"]
["TECHNIK","HTN  3,2/30 černá"]
["TECHNIK","HTN  3,2/30 modrá"]
["TECHNIK","HTN  3,2/30 rudá"]
["TECHNIK","HTN  3,2/30 šedá"]
["TECHNIK","HTN  3,2/30 transp"]
["TECHNIK","HTN  3,2/30 žlutá"]
["TECHNIK","HTN  3,2/30 žz"]
["TECHNIK","HTN  4,8/20 bílá"]
["TECHNIK","HTN  4,8/20 černá"]
["TECHNIK","HTN  4,8/20 modrá"]
["TECHNIK","HTN  4,8/20 rudá"]
["TECHNIK","HTN  4,8/20 transp"]
["TECHNIK","HTN  4,8/20 zelená"]
["TECHNIK","HTN  4,8/20 žlutá"]
["TECHNIK","HTN  4,8/30 bílá"]
["TECHNIK","HTN  4,8/30 černá"]
["TECHNIK","HTN  4,8/30 hnědá"]
["TECHNIK","HTN  4,8/30 modrá"]
["TECHNIK","HTN  4,8/30 rudá"]
["TECHNIK","HTN  4,8/30 šedá"]
["TECHNIK","HTN  4,8/30 transp"]
["TECHNIK","HTN  4,8/30 žlutá"]
["TECHNIK","HTN  4,8/30 žz"]
["TECHNIK","HTN  6,4/20 bílá"]
["TECHNIK","HTN  6,4/20 černá"]
["TECHNIK","HTN  6,4/20 modrá"]
["TECHNIK","HTN  6,4/20 rudá"]
["TECHNIK","HTN  6,4/20 zelená"]
["TECHNIK","HTN  6,4/20 žlutá"]
["TECHNIK","HTN  6,4/30 bílá"]
["TECHNIK","HTN  6,4/30 černá"]
["TECHNIK","HTN  6,4/30 modrá"]
["TECHNIK","HTN  6,4/30 rudá"]
["TECHNIK","HTN  6,4/30 šedá"]
["TECHNIK","HTN  6,4/30 transp"]
["TECHNIK","HTN  6,4/30 žlutá"]
["TECHNIK","HTN  6,4/30 žz"]
["TECHNIK","HTN  9,5/20 bílá"]
["TECHNIK","HTN  9,5/20 černá"]
["TECHNIK","HTN  9,5/20 modrá"]
["TECHNIK","HTN  9,5/20 rudá"]
["TECHNIK","HTN  9,5/20 zelená"]
["TECHNIK","HTN  9,5/20 žlutá"]
["TECHNIK","HTN  9,5/30 černá"]
["TECHNIK","HTN  9,5/30 modrá"]
["TECHNIK","HTN  9,5/30 rudá"]
["TECHNIK","HTN  9,5/30 šedá"]
["TECHNIK","HTN  9,5/30 transp"]
["TECHNIK SPECIAL - AKCIA","HT-TC 026"]
["TECHNIK SPECIAL - AKCIA","HT-TC 026 Y"]
["TECHNIK SPECIAL - AKCIA","HT-TC 041"]
["TECHNIK SPECIAL - AKCIA","HT-TC 051"]
["TECHNIK SPECIAL - AKCIA","HT-TC 055"]
["TECHNIK SPECIAL - AKCIA","HT-TC 065"]
["TECHNIK SPECIAL - AKCIA","HT-TC 0851"]
["TECHNIK","HX 1"]
["TECHNIK","HX 1/TF"]
["TECHNIK","HX 2"]
["TECHNIK","HX 3"]
["TECHNIK","HX 4"]
["TECHNIK","HX 5"]
["TECHNIK","HX 6"]
["TECHNIK","HX 7"]
["TECHNIK","HX 8"]
["TECHNIK","HX 9"]
["TECHNIK","HXKT  3,2/0,8"]
["TECHNIK","HXKT  4,8/1,5"]
["TECHNIK","HXKT  6,4/1,9"]
["TECHNIK","HXKT  9,5/3,4"]
["TECHNIK","HXKT 12,7/5"]
["TECHNIK","HXKT 19/8"]
["TECHNIK","HXKT 25,4/10,2"]
["TECHNIK SPECIAL - AKCIA","HYDR. RED 19x40/9,5"]
["TECHNIK SPECIAL - AKCIA","HYDR. RYCHLOSP. G1/4"]
["TECHNIK SPECIAL - AKCIA","HYDR. RYCHLOSP. R1/4"]
["TECHNIK SPECIAL - AKCIA","HYDR. ŠROUB  6"]
["TECHNIK SPECIAL - AKCIA","HYDR. ŠROUB  9,5"]
["TECHNIK SPECIAL - AKCIA","HYDR. ŠROUB 11,1"]
["TECHNIK SPECIAL - AKCIA","HYDR. ŠROUB 19"]
["TECHNIK SPECIAL - AKCIA","HYDR. ŠROUB 19x 6"]
["TECHNIK SPECIAL - AKCIA","HYDR. ŠROUB 19x 9,5"]
["TECHNIK SPECIAL - AKCIA","HYDR. ŠROUB 19x 9,5P"]
["TECHNIK SPECIAL - AKCIA","HYDR. ŠROUB 19x11,1"]
["TECHNIK SPECIAL - AKCIA","HYDR. ŠROUB 19x11,1P"]
["TECHNIK SPECIAL - AKCIA","HYDR. ŠROUBENÍ G1/4"]
["TECHNIK","Chladící sprej"]
["TECHNIK","Chrom sprej"]
["TECHNIK","I3000  3,2/1,0 oranž"]
["TECHNIK","I3000  6,4/2,0 žlutá"]
["TECHNIK","I3000 12,7/4,0 oranž"]
["TECHNIK","I3000 25,4/8,0 žlutá"]
["TECHNIK","IAKT  3/1"]
["TECHNIK","IAKT  3/1 ."]
["TECHNIK","IAKT  3/1 R300"]
["TECHNIK","IAKT  3/1 transp"]
["TECHNIK","IAKT  4,5/1,5"]
["TECHNIK","IAKT  4,5/1,5 ."]
["TECHNIK","IAKT  4,5/1,5 transp"]
["TECHNIK","IAKT  4,5/1,5.R100"]
["TECHNIK","IAKT  4,5/1,5.R75"]
["TECHNIK","IAKT  4/1"]
["TECHNIK","IAKT  4/1 ."]
["TECHNIK","IAKT  4/1 R300"]
["TECHNIK","IAKT  4/1 transp"]
["TECHNIK","IAKT  6/2"]
["TECHNIK","IAKT  6/2 ."]
["TECHNIK","IAKT  6/2 R300"]
["TECHNIK","IAKT  6/2 transp"]
["TECHNIK","IAKT  6/2 transpR300"]
["TECHNIK","IAKT  8/2"]
["TECHNIK","IAKT  8/2 ."]
["TECHNIK","IAKT  8/2 transp"]
["TECHNIK","IAKT  9/3"]
["TECHNIK","IAKT  9/3 ."]
["TECHNIK","IAKT  9/3 R150"]
["TECHNIK","IAKT  9/3 transp"]
["TECHNIK","IAKT  9/3 transpR150"]
["TECHNIK","IAKT 12/3"]
["TECHNIK","IAKT 12/3 ."]
["TECHNIK","IAKT 12/3 R100"]
["TECHNIK","IAKT 12/3 transp"]
["TECHNIK","IAKT 12/3 transpR100"]
["TECHNIK","IAKT 12/4"]
["TECHNIK","IAKT 12/4 ."]
["TECHNIK","IAKT 12/4 transp"]
["TECHNIK","IAKT 12/4 transpR100"]
["TECHNIK","IAKT 16/4"]
["TECHNIK","IAKT 16/4 ."]
["TECHNIK","IAKT 16/4 R50"]
["TECHNIK","IAKT 16/4 transp"]
["TECHNIK","IAKT 16/4 transp R75"]
["TECHNIK","IAKT 19/6"]
["TECHNIK","IAKT 19/6 ."]
["TECHNIK","IAKT 19/6 R50"]
["TECHNIK","IAKT 19/6 transp"]
["TECHNIK","IAKT 24/6"]
["TECHNIK","IAKT 24/6 ."]
["TECHNIK","IAKT 24/6 transp"]
["TECHNIK","IAKT 24/8"]
["TECHNIK","IAKT 24/8 ."]
["TECHNIK","IAKT 24/8 transp"]
["TECHNIK","IAKT 32/8"]
["TECHNIK","IAKT 32/8 ."]
["TECHNIK","IAKT 32/8 R50"]
["TECHNIK","IAKT 32/8 transp"]
["TECHNIK","IAKT 40/13"]
["TECHNIK","IAKT 40/13 ."]
["TECHNIK","IAKT 40/13 transp"]
["TECHNIK","IAKT 52/13"]
["TECHNIK","IAKT 52/13 ."]
["TECHNIK","IAKT 52/13 R30"]
["TECHNIK","IAKT 52/13 transp"]
["TECHNIK","ID 25x15"]
["TECHNIK","ID 40x20"]
["TECHNIK","ID 60x25"]
["TECHNIK","ID 60x50"]
["TECHNIK","ID 90x20"]
["TECHNIK","IDM 60x25"]
["TECHNIK","IDM120x50"]
["TECHNIK","IDST 50x10"]
["TECHNIK","IDST 65x10"]
["TECHNIK","IDST 90x10"]
["TECHNIK","IDST 90x20"]
["TECHNIK","IDST100x10"]
["TECHNIK","IDST130x10"]
["TECHNIK","IDST150x10"]
["TECHNIK","IDZ 30x 8"]
["TECHNIK","IDZ 40x15"]
["TECHNIK","IDZ 50x10"]
["TECHNIK","IDZ 60x25"]
["TECHNIK","IDZ KL 50x20"]
["TECHNIK","IDZ UNI 50x20"]
["TECHNIK","IT 120 - CC 2"]
["TECHNIK","IT 120 - Luxmetr B"]
["TECHNIK","IT 120 - Uzemnění"]
["TECHNIK","IT 120B"]
["TECHNIK","JOKARI  6"]
["TECHNIK","JOKARI  6N"]
["TECHNIK","JOKARI 10280"]
["TECHNIK","JOKARI 10282"]
["TECHNIK","JOKARI 16"]
["TECHNIK","JOKARI 30010"]
["TECHNIK","JOKARI 30140"]
["TECHNIK","JOKARI 30155"]
["TECHNIK","JOKARI ESD PLUS 001"]
["TECHNIK","JOKARI Q"]
["TECHNIK","JOKARI Q SET"]
["TECHNIK SPECIAL - AKCIA","JQ 6100"]
["TECHNIK","JT 539T"]
["TECHNIK SPECIAL - AKCIA","K 18"]
["TECHNIK SPECIAL - AKCIA","K 18 L"]
["TECHNIK SPECIAL - AKCIA","K 22"]
["TECHNIK SPECIAL - AKCIA","K 22 L"]
["TECHNIK","KAOB  3"]
["TECHNIK","KAOB  5"]
["TECHNIK","KAOB  6"]
["TECHNIK","KAOB  8"]
["TECHNIK","KAOB 10"]
["TECHNIK","KAOB 13"]
["TECHNIK","KAOB 16"]
["TECHNIK","KAOB 19"]
["TECHNIK","KAOB 25"]
["TECHNIK","KAOB 28"]
["TECHNIK","KAOB 37"]
["TECHNIK","KAOBC  3"]
["TECHNIK","KAOBC  6"]
["TECHNIK","KAOBC  7"]
["TECHNIK","KAOBC  8"]
["TECHNIK","KAOBC 10"]
["TECHNIK","KAOBC 28"]
["TECHNIK","KAOBF  8"]
["TECHNIK","KAOBFE 1204"]
["TECHNIK","KAOBFE 1205"]
["TECHNIK","KAOBFE 1206"]
["TECHNIK","KAOBFE 1206 N"]
["TECHNIK","KAOBFE 1208"]
["TECHNIK","KAOBFE 1210"]
["TECHNIK","KAOBFE 1210 N"]
["TECHNIK","KAOBFE 1212"]
["TECHNIK","KAOBFE 1214"]
["TECHNIK","KAOBFE 1214 N"]
["TECHNIK","KAOBFE 1216"]
["TECHNIK","KAOBFE 1219"]
["TECHNIK","KAOBFE 1532"]
["TECHNIK","KAOBFE 1538"]
["TECHNIK","KAOH  3,5"]
["TECHNIK","KAOH  5"]
["TECHNIK","KAOH  5 šedá"]
["TECHNIK","KAOH  7"]
["TECHNIK","KAOH  7 šedá"]
["TECHNIK","KAOH  9"]
["TECHNIK","KAOH  9 šedá"]
["TECHNIK","KAOH 11"]
["TECHNIK","KAOH 11 šedá"]
["TECHNIK","KAOH 14"]
["TECHNIK","KAOH 18"]
["TECHNIK","KAOH 6/2"]
["TECHNIK","KAOH10/2"]
["TECHNIK","KAP 12x12"]
["TECHNIK","KAP 19x19"]
["TECHNIK","KAP 19x19/2"]
["TECHNIK","KAP 20x20"]
["TECHNIK","KAP 25x25."]
["TECHNIK","KAP 25x32"]
["TECHNIK","KAP 27x27/3M"]
["TECHNIK","KAP 28x28"]
["TECHNIK","KAP 28x28/2"]
["TECHNIK","KAP 30x30"]
["TECHNIK","KAP 40x40"]
["TECHNIK","KAPC 12x12"]
["TECHNIK","KAPC 19x19"]
["TECHNIK","KAPC 19x19/2"]
["TECHNIK","KAPC 25x32"]
["TECHNIK","KAPC 27x27/3M"]
["TECHNIK","KAPC 28x28"]
["TECHNIK","KAPC 28x28/2"]
["TECHNIK","KAPH 5"]
["TECHNIK","KAPH 6"]
["TECHNIK","KAPH 8"]
["TECHNIK","KAPH 9"]
["TECHNIK","KAPO 4"]
["TECHNIK","KAPO 8"]
["TECHNIK","KAPP 15x25"]
["TECHNIK","KAPP 20x25"]
["TECHNIK","KAPP 25x25"]
["TECHNIK","KAPP 30x25"]
["TECHNIK","KAPS 4/4"]
["TECHNIK","KAPS 4/5"]
["TECHNIK","KAPS 5"]
["TECHNIK","KAPS 5/4,5"]
["TECHNIK","KAPS 9"]
["TECHNIK","KAPS 9/4,5"]
["TECHNIK","KAPS 9/5"]
["TECHNIK","KAPSC 5"]
["TECHNIK","KAPSC 5/4,5"]
["TECHNIK","KAPSC 9"]
["TECHNIK","KAPSC 9/4,5"]
["TECHNIK","KAS 10"]
["TECHNIK","KAS 15"]
["TECHNIK","KAS 20"]
["TECHNIK","KES 2x2,5"]
["TECHNIK","KES 3x2,5"]
["TECHNIK","KES 4x2,5"]
["TECHNIK","KES 5x2,5"]
["TECHNIK","KES 6x2,5"]
["TECHNIK","KES 8x2,5"]
["TECHNIK","KI 0,5- 8/PA"]
["TECHNIK","KI 0,5-10"]
["TECHNIK","KI 1,5- 8"]
["TECHNIK","KI 1,5- 8/E"]
["TECHNIK","KI 1,5- 8/PA"]
["TECHNIK","KI 1,5- 8/PC"]
["TECHNIK","KI 1,5-10"]
["TECHNIK","KI 1,5-10/E"]
["TECHNIK","KI 1,5-10/PA"]
["TECHNIK","KI 1,5-10/PC"]
["TECHNIK","KI 1,5-12"]
["TECHNIK","KI 1,5-12/E"]
["TECHNIK","KI 1,5-12/PC"]
["TECHNIK","KI 1,5-12/PK"]
["TECHNIK","KI 1,5-16"]
["TECHNIK","KI 2,5- 8"]
["TECHNIK","KI 2,5- 8/PC"]
["TECHNIK","KI 2,5-10"]
["TECHNIK","KI 2,5-10/E"]
["TECHNIK","KI 2,5-12"]
["TECHNIK","KI 2,5-12/E"]
["TECHNIK","KI 2,5-12/PC"]
["TECHNIK","KI 2,5-17"]
["TECHNIK","KI 2,5-17/PC"]
["TECHNIK","KI 6-10"]
["TECHNIK","KI 6-12"]
["TECHNIK","KI 6-14"]
["TECHNIK","KI 6-14/E"]
["TECHNIK","KI 6-14/PC"]
["TECHNIK","KI10-12"]
["TECHNIK","KI10-12."]
["TECHNIK","KI16-14"]
["TECHNIK","KI16-14."]
["TECHNIK","KI25-16"]
["TECHNIK","KI25-16."]
["TECHNIK","KI35-20"]
["TECHNIK","KI35-20."]
["TECHNIK","KI50-26"]
["TECHNIK","KI70-31"]
["TECHNIK","KI95-31"]
["TECHNIK","KIPL 0,5- 8"]
["TECHNIK","KIPL 1,5-12"]
["TECHNIK","KIPL 1,5-18"]
["TECHNIK","KIPL 2,5-12"]
["TECHNIK","KIPL 2,5-18"]
["TECHNIK","KIPL 6-12"]
["TECHNIK","KIPL 6-16"]
["TECHNIK","KIPPL 1,5/30"]
["TECHNIK","KIPPL 1,5/46"]
["TECHNIK","KIPPL 2,5/30"]
["TECHNIK","KIPPL 2,5/46"]
["TECHNIK","KIPPL 6/30"]
["TECHNIK","KIPPL 6/46"]
["TECHNIK","KK 2,5-3,5"]
["TECHNIK","KK 2,5-4"]
["TECHNIK","KKC 1,5-4/PA"]
["TECHNIK","KKC 1,5-4/PC"]
["TECHNIK","KKC 2,5-4/PC"]
["TECHNIK","KKP 1,5-4"]
["TECHNIK","KKP 1,5-4/PA"]
["TECHNIK","KKP 1,5-4/PC"]
["TECHNIK","KKP 2,5-4"]
["TECHNIK","KKP 2,5-4/PC"]
["TECHNIK","KKP 2,5-5"]
["TECHNIK","KKP 2,5-5/PC"]
["TECHNIK","KKP 6-5"]
["TECHNIK","KKP 6-5/PC"]
["TECHNIK","KKSN 2,5-3,5"]
["TECHNIK","KKSN 2,5-4"]
["TECHNIK","KL 01"]
["TECHNIK","KLE 2,5"]
["TECHNIK","KLS 0,14-1,5"]
["TECHNIK","KN   0,5-10"]
["TECHNIK","KN   1,5- 8"]
["TECHNIK","KN   1,5-10"]
["TECHNIK","KN   1,5-12"]
["TECHNIK","KN   1,5-16"]
["TECHNIK","KN   2,5- 8"]
["TECHNIK","KN   2,5-10"]
["TECHNIK","KN   2,5-12"]
["TECHNIK","KN   2,5-16"]
["TECHNIK","KN   6-10"]
["TECHNIK","KN   6-12"]
["TECHNIK","KN   6-14"]
["TECHNIK","KN  10"]
["TECHNIK","KN  16"]
["TECHNIK","KN  25"]
["TECHNIK","KN  35"]
["TECHNIK","KN  50"]
["TECHNIK","KN  70"]
["TECHNIK","KN  95"]
["TECHNIK","KN 00 11 01"]
["TECHNIK","KN 00 11 02"]
["TECHNIK","KN 00 11 03"]
["TECHNIK","KN 00 20 17"]
["TECHNIK","KN 00 21 01 TL"]
["TECHNIK","KN 00 21 02 LE"]
["TECHNIK","KN 00 21 02 SL"]
["TECHNIK","KN 00 21 05 LE"]
["TECHNIK","KN 00 21 20 LE"]
["TECHNIK","KN 00 21 40 LE"]
["TECHNIK","KN 00 21 41 LE"]
["TECHNIK","KN 02 01 180"]
["TECHNIK","KN 02 01 200"]
["TECHNIK","KN 02 02 180"]
["TECHNIK","KN 02 02 200"]
["TECHNIK","KN 02 06 180"]
["TECHNIK","KN 02 06 200"]
["TECHNIK","KN 03 01 160"]
["TECHNIK","KN 03 01 180"]
["TECHNIK","KN 03 01 200"]
["TECHNIK","KN 03 02 160"]
["TECHNIK","KN 03 02 180"]
["TECHNIK","KN 03 02 200"]
["TECHNIK","KN 03 06 160"]
["TECHNIK","KN 03 06 180"]
["TECHNIK","KN 03 06 200"]
["TECHNIK","KN 08 05 110"]
["TECHNIK","KN 11 01 160"]
["TECHNIK","KN 11 02 160"]
["TECHNIK","KN 11 06 160"]
["TECHNIK","KN 11 92 140"]
["TECHNIK","KN 12 62 180"]
["TECHNIK","KN 12 80 100 SB"]
["TECHNIK","KN 13 01 160"]
["TECHNIK","KN 13 02 160"]
["TECHNIK","KN 13 05 160"]
["TECHNIK","KN 13 81 200"]
["TECHNIK","KN 13 96 200"]
["TECHNIK","KN 14 22 160"]
["TECHNIK","KN 14 26 160"]
["TECHNIK","KN 16 20 165 SB"]
["TECHNIK","KN 16 29 165"]
["TECHNIK","KN 16 60 05 SB"]
["TECHNIK","KN 16 60 100 SB"]
["TECHNIK","KN 16 65 125 SB"]
["TECHNIK","KN 16 80 125 SB"]
["TECHNIK","KN 16 85 125 SB"]
["TECHNIK","KN 19 01 130"]
["TECHNIK","KN 19 03 130"]
["TECHNIK","KN 20 02 160"]
["TECHNIK","KN 22 01 160"]
["TECHNIK","KN 22 01 180"]
["TECHNIK","KN 22 02 160"]
["TECHNIK","KN 22 06 160"]
["TECHNIK","KN 22 07 160"]
["TECHNIK","KN 23 01 140"]
["TECHNIK","KN 25 01 160"]
["TECHNIK","KN 25 02 140"]
["TECHNIK","KN 25 02 160"]
["TECHNIK","KN 25 06 160"]
["TECHNIK","KN 25 25 160"]
["TECHNIK","KN 25 26 160"]
["TECHNIK","KN 26 11 200"]
["TECHNIK","KN 26 12 200"]
["TECHNIK","KN 26 16 200"]
["TECHNIK","KN 26 21 200"]
["TECHNIK","KN 26 22 200"]
["TECHNIK","KN 26 26 200"]
["TECHNIK","KN 26 27 200"]
["TECHNIK","KN 29 25 160"]
["TECHNIK","KN 30 11 160"]
["TECHNIK","KN 30 11 190"]
["TECHNIK","KN 30 15 160"]
["TECHNIK","KN 30 15 190"]
["TECHNIK","KN 30 16 160"]
["TECHNIK","KN 30 25 140"]
["TECHNIK","KN 30 31 160"]
["TECHNIK","KN 30 35 160"]
["TECHNIK","KN 30 36 160"]
["TECHNIK","KN 31 11 160"]
["TECHNIK","KN 31 25 160"]
["TECHNIK","KN 33 01 160"]
["TECHNIK","KN 35 12 115"]
["TECHNIK","KN 35 22 115"]
["TECHNIK","KN 35 32 115"]
["TECHNIK","KN 35 42 115"]
["TECHNIK","KN 35 62 145"]
["TECHNIK","KN 38 15 200"]
["TECHNIK","KN 38 71 200"]
["TECHNIK SPECIAL - AKCIA","KN 40"]
["TECHNIK","KN 40 04 180"]
["TECHNIK","KN 44 11 J0"]
["TECHNIK","KN 44 11 J1"]
["TECHNIK","KN 44 11 J2"]
["TECHNIK","KN 44 11 J3"]
["TECHNIK","KN 44 11 J4"]
["TECHNIK","KN 44 21 J01"]
["TECHNIK","KN 44 21 J11"]
["TECHNIK","KN 44 21 J21"]
["TECHNIK","KN 44 21 J31"]
["TECHNIK","KN 44 21 J41"]
["TECHNIK","KN 46 11 A0"]
["TECHNIK","KN 46 11 A1"]
["TECHNIK","KN 46 11 A2"]
["TECHNIK","KN 46 11 A3"]
["TECHNIK","KN 46 11 A4"]
["TECHNIK","KN 46 21 A01"]
["TECHNIK","KN 46 21 A11"]
["TECHNIK","KN 46 21 A21"]
["TECHNIK","KN 46 21 A31"]
["TECHNIK","KN 46 21 A41"]
["TECHNIK","KN 50 01 180"]
["TECHNIK","KN 50 01 210"]
["TECHNIK","KN 50 01 225"]
["TECHNIK","KN 50 01 250"]
["TECHNIK","KN 51 01 210"]
["TECHNIK","KN 61 01 200"]
["TECHNIK","KN 62 12 120"]
["TECHNIK","KN 64 11 115"]
["TECHNIK","KN 64 12 115 ESD"]
["TECHNIK","KN 64 32 120"]
["TECHNIK","KN 64 52 115"]
["TECHNIK","KN 64 62 120"]
["TECHNIK SPECIAL - AKCIA","KN 65"]
["TECHNIK","KN 67 01 200"]
["TECHNIK","KN 67 05 200"]
["TECHNIK","KN 70 01 140"]
["TECHNIK","KN 70 01 160"]
["TECHNIK","KN 70 01 180"]
["TECHNIK","KN 70 02 140"]
["TECHNIK","KN 70 02 160"]
["TECHNIK","KN 70 02 180"]
["TECHNIK","KN 70 05 160"]
["TECHNIK","KN 70 06 140"]
["TECHNIK","KN 70 06 160"]
["TECHNIK","KN 70 06 180"]
["TECHNIK","KN 70 07 160"]
["TECHNIK","KN 70 07 180"]
["TECHNIK","KN 70 11 110"]
["TECHNIK","KN 70 26 160"]
["TECHNIK","KN 71 02 200"]
["TECHNIK","KN 71 41 200"]
["TECHNIK","KN 72 01 140"]
["TECHNIK","KN 72 01 160"]
["TECHNIK","KN 72 02 125"]
["TECHNIK","KN 72 11 160"]
["TECHNIK","KN 72 51 160"]
["TECHNIK","KN 73 72 180"]
["TECHNIK","KN 74 01 180"]
["TECHNIK","KN 74 01 200"]
["TECHNIK","KN 74 02 160"]
["TECHNIK","KN 74 02 180"]
["TECHNIK","KN 74 02 200"]
["TECHNIK","KN 74 06 160"]
["TECHNIK","KN 74 06 180"]
["TECHNIK","KN 74 06 250"]
["TECHNIK","KN 74 12 180"]
["TECHNIK","KN 74 22 200"]
["TECHNIK","KN 75 22 125"]
["TECHNIK","KN 75 52 125"]
["TECHNIK","KN 76 05 125"]
["TECHNIK","KN 76 12 125"]
["TECHNIK","KN 76 22 125"]
["TECHNIK","KN 77 01 115"]
["TECHNIK","KN 77 02 115"]
["TECHNIK","KN 77 02 130"]
["TECHNIK","KN 77 21 115"]
["TECHNIK","KN 77 21 130"]
["TECHNIK","KN 77 22 115"]
["TECHNIK","KN 77 22 115 ESD"]
["TECHNIK","KN 77 22 130"]
["TECHNIK","KN 77 32 115"]
["TECHNIK","KN 77 42 115"]
["TECHNIK","KN 77 72 115"]
["TECHNIK","KN 78 03 125"]
["TECHNIK","KN 78 13 125"]
["TECHNIK","KN 78 61 125"]
["TECHNIK SPECIAL - AKCIA","KN 85"]
["TECHNIK","KN 85 01 250"]
["TECHNIK","KN 85 51 250A"]
["TECHNIK","KN 86 03 125"]
["TECHNIK","KN 86 03 150"]
["TECHNIK","KN 86 03 180"]
["TECHNIK","KN 86 03 250"]
["TECHNIK","KN 86 03 300"]
["TECHNIK","KN 86 03 400"]
["TECHNIK","KN 86 05 150"]
["TECHNIK","KN 86 05 180"]
["TECHNIK","KN 86 05 250"]
["TECHNIK","KN 86 07 250"]
["TECHNIK","KN 87 01 125"]
["TECHNIK","KN 87 01 150"]
["TECHNIK","KN 87 01 180"]
["TECHNIK","KN 87 01 250"]
["TECHNIK","KN 87 01 300"]
["TECHNIK","KN 87 01 400"]
["TECHNIK","KN 87 01 560"]
["TECHNIK","KN 87 02 180"]
["TECHNIK","KN 87 02 250"]
["TECHNIK","KN 87 02 300"]
["TECHNIK","KN 87 05 250"]
["TECHNIK","KN 87 05 300"]
["TECHNIK","KN 87 26 250"]
["TECHNIK","KN 87 51 250"]
["TECHNIK","KN 88 01 180"]
["TECHNIK","KN 88 01 250"]
["TECHNIK","KN 88 01 300"]
["TECHNIK","KN 88 02 180"]
["TECHNIK","KN 88 02 250"]
["TECHNIK","KN 88 02 300"]
["TECHNIK","KN 88 06 250"]
["TECHNIK","KN 92 02 53"]
["TECHNIK","KN 92 22 07"]
["TECHNIK","KN 92 27 61"]
["TECHNIK","KN 92 27 62"]
["TECHNIK","KN 92 28 69 ESD"]
["TECHNIK","KN 92 37 64"]
["TECHNIK","KN 92 38 75 ESD"]
["TECHNIK","KN 95 03 160 SB"]
["TECHNIK","KN 95 05 140"]
["TECHNIK","KN 95 05 165"]
["TECHNIK","KN 95 06 230"]
["TECHNIK","KN 95 11 165"]
["TECHNIK","KN 95 12 165"]
["TECHNIK","KN 95 12 200"]
["TECHNIK","KN 95 16 165"]
["TECHNIK","KN 95 17 200"]
["TECHNIK","KN 95 22 165"]
["TECHNIK","KN 95 26 165"]
["TECHNIK","KN 95 61 190"]
["TECHNIK","KN 97 21 215"]
["TECHNIK","KN 97 21 215B"]
["TECHNIK","KN 97 21 215C"]
["TECHNIK","KN 97 50 01"]
["TECHNIK","KN 97 51 10"]
["TECHNIK","KN 97 51 12"]
["TECHNIK","KN 97 52 05"]
["TECHNIK","KN 97 52 06"]
["TECHNIK","KN 97 52 08"]
["TECHNIK","KN 97 52 09"]
["TECHNIK","KN 97 52 13"]
["TECHNIK","KN 97 52 20"]
["TECHNIK","KN 97 53 09"]
["TECHNIK","KN 97 61 145F"]
["TECHNIK","KN 97 90 00"]
["TECHNIK","KN 97 90 00 LE"]
["TECHNIK","KN 97 90 01"]
["TECHNIK","KN 97 90 05"]
["TECHNIK","KN 97 90 06"]
["TECHNIK","KN 97 90 09"]
["TECHNIK","KN 97 90 10"]
["TECHNIK","KN 97 90 12"]
["TECHNIK","KN 97 90 21"]
["TECHNIK","KN 97 90 22"]
["TECHNIK","KN 97 90 23"]
["TECHNIK","KN 97 90 24"]
["TECHNIK","KN 97 90 25"]
["TECHNIK","KN 98 00 08"]
["TECHNIK","KN 98 00 10"]
["TECHNIK","KN 98 00 12"]
["TECHNIK","KN 98 00 17"]
["TECHNIK","KN 98 00 18"]
["TECHNIK","KN 98 00 19"]
["TECHNIK","KN 98 00 22"]
["TECHNIK","KN 98 00 24"]
["TECHNIK","KN 98 00 27"]
["TECHNIK","KN 98 01 13"]
["TECHNIK","KN 98 01 17"]
["TECHNIK","KN 98 03 055"]
["TECHNIK","KN 98 03 07"]
["TECHNIK","KN 98 03 08"]
["TECHNIK","KN 98 03 10"]
["TECHNIK","KN 98 14 05"]
["TECHNIK","KN 98 14 06"]
["TECHNIK","KN 98 14 08"]
["TECHNIK","KN 98 20 10"]
["TECHNIK","KN 98 20 25"]
["TECHNIK","KN 98 20 30"]
["TECHNIK","KN 98 20 35"]
["TECHNIK","KN 98 20 40"]
["TECHNIK","KN 98 20 55"]
["TECHNIK","KN 98 20 65"]
["TECHNIK","KN 98 20 80"]
["TECHNIK","KN 98 24 00"]
["TECHNIK","KN 98 24 01"]
["TECHNIK","KN 98 24 02"]
["TECHNIK","KN 98 24 03"]
["TECHNIK","KN 98 24 04"]
["TECHNIK","KN 98 39 06"]
["TECHNIK","KN 98 40"]
["TECHNIK","KN 98 41"]
["TECHNIK","KN 98 42"]
["TECHNIK","KN 98 43 50"]
["TECHNIK","KN 98 45 125"]
["TECHNIK","KN 98 45 250"]
["TECHNIK","KN 98 47 10"]
["TECHNIK","KN 98 47 11"]
["TECHNIK","KN 98 47 12"]
["TECHNIK","KN 98 47 13"]
["TECHNIK","KN 98 47 14"]
["TECHNIK","KN 98 47 16"]
["TECHNIK","KN 98 47 17"]
["TECHNIK","KN 98 47 18"]
["TECHNIK","KN 98 47 19"]
["TECHNIK","KN 98 47 22"]
["TECHNIK","KN 98 47 24"]
["TECHNIK","KN 98 47 27"]
["TECHNIK","KN 98 49 05"]
["TECHNIK","KN 98 49 06"]
["TECHNIK","KN 98 49 08"]
["TECHNIK","KN 98 65 40"]
["TECHNIK","KN 98 65 41"]
["TECHNIK","KN 98 99 11"]
["TECHNIK","KN 98 99 12"]
["TECHNIK","KN 98 99 13"]
["TECHNIK","KNPL 0,5- 8"]
["TECHNIK","KNPL 1,5-10"]
["TECHNIK","KNPL 1,5-14"]
["TECHNIK","KNPL 1,5-18"]
["TECHNIK","KNPL 2,5-10"]
["TECHNIK","KNPL 2,5-14"]
["TECHNIK","KNPL 2,5-18"]
["TECHNIK","KNPL 6-10"]
["TECHNIK","KNPL 6-14"]
["TECHNIK","KNPL 6-18"]
["TECHNIK SPECIAL - AKCIA","KNZ 32/48"]
["TECHNIK SPECIAL - AKCIA","KNZ 32/48 razník"]
["TECHNIK","KO 2,5-3,5"]
["TECHNIK","KO 2,5-4"]
["TECHNIK","KOSN 2,5-3,5"]
["TECHNIK","KOSN 2,5-4"]
["TECHNIK","KPC 1,5-68/PA"]
["TECHNIK","KPC 2,5-68/PA"]
["TECHNIK","KPC 6-68/PA"]
["TECHNIK","KPP 1,5-25"]
["TECHNIK","KPP 1,5-25/PC"]
["TECHNIK","KPP 1,5-28"]
["TECHNIK","KPP 1,5-28/PC"]
["TECHNIK","KPP 1,5-45"]
["TECHNIK","KPP 1,5-45/PC"]
["TECHNIK","KPP 1,5-48"]
["TECHNIK","KPP 1,5-48/PA"]
["TECHNIK","KPP 1,5-48/PC"]
["TECHNIK","KPP 1,5-68"]
["TECHNIK","KPP 1,5-68/PA"]
["TECHNIK","KPP 1,5-68/PC"]
["TECHNIK","KPP 2,5-45"]
["TECHNIK","KPP 2,5-45/PC"]
["TECHNIK","KPP 2,5-48"]
["TECHNIK","KPP 2,5-48/PA"]
["TECHNIK","KPP 2,5-48/PC"]
["TECHNIK","KPP 2,5-68"]
["TECHNIK","KPP 2,5-68/PA"]
["TECHNIK","KPP 2,5-68/PC"]
["TECHNIK","KPP 6-68"]
["TECHNIK","KPP 6-68/PA"]
["TECHNIK","KPP 6-68/PC"]
["TECHNIK","KPPS 1,5-25"]
["TECHNIK","KPPS 1,5-28"]
["TECHNIK","KPPS 1,5-45"]
["TECHNIK","KPPS 1,5-48"]
["TECHNIK","KPPS 1,5-68"]
["TECHNIK","KPPS 2,5-45"]
["TECHNIK","KPPS 2,5-48"]
["TECHNIK","KPPS 2,5-68"]
["TECHNIK","KPPS 6-68"]
["TECHNIK","KRJ 45 bílá"]
["TECHNIK","KRJ 45 černá"]
["TECHNIK","KRJ 45 modrá"]
["TECHNIK","KRJ 45 rudá"]
["TECHNIK","KRJ 45 šedá"]
["TECHNIK","KRJ 45 zelená"]
["TECHNIK","KRJ 45 žlutá"]
["TECHNIK","KRJ 45V bílá"]
["TECHNIK","KRJ 45V černá"]
["TECHNIK","KRJ 45V modrá"]
["TECHNIK","KRJ 45V rudá"]
["TECHNIK","KRJ 45V šedá"]
["TECHNIK","KRJ 45V zelená"]
["TECHNIK","KRJ 45V žlutá"]
["TECHNIK","KS  5"]
["TECHNIK","KS  8"]
["TECHNIK","KS 11"]
["TECHNIK","KS 15"]
["TECHNIK","KS 160/1000"]
["TECHNIK","KS 18"]
["TECHNIK","KS 24"]
["TECHNIK","KSU 12"]
["TECHNIK","KSU 12 G"]
["TECHNIK","KSU 14"]
["TECHNIK","KSU 19"]
["TECHNIK","KSU 23"]
["TECHNIK","KSUC  6"]
["TECHNIK","KSUC  9"]
["TECHNIK","KSUC 12"]
["TECHNIK","KSUC 14"]
["TECHNIK","KSUC 16"]
["TECHNIK","KSUC 18"]
["TECHNIK","KSUS  7"]
["TECHNIK","KSUS  8"]
["TECHNIK","KSUS 10"]
["TECHNIK","KSUS 14"]
["TECHNIK","KSUS 18"]
["TECHNIK","KT  40/15"]
["TECHNIK","KT 28  PA"]
["TECHNIK","KT 28 bílá"]
["TECHNIK","KT 28 černá"]
["TECHNIK","KT 28 modrá"]
["TECHNIK","KT 28 PVC černá"]
["TECHNIK","KT 28 PVC modrá"]
["TECHNIK","KT 28 PVC rudá"]
["TECHNIK","KT 28 PVC transp"]
["TECHNIK","KT 28 rudá"]
["TECHNIK","KT 28 žlutá"]
["TECHNIK","KT 48  PA"]
["TECHNIK","KT 48  PVC černá"]
["TECHNIK","KT 48  PVC modrá"]
["TECHNIK","KT 48  PVC rudá"]
["TECHNIK","KT 48  PVC transp"]
["TECHNIK","KT 48  PVC žlutá"]
["TECHNIK","KT 48 bílá"]
["TECHNIK","KT 48 černá"]
["TECHNIK","KT 48 modrá"]
["TECHNIK","KT 48 rudá"]
["TECHNIK","KT 48 žlutá"]
["TECHNIK","KT 68  PA"]
["TECHNIK","KT 68  PA černá"]
["TECHNIK","KT 68  PVC černá"]
["TECHNIK","KT 68  PVC modrá"]
["TECHNIK","KT 68  PVC rudá"]
["TECHNIK","KT 68  PVC transp"]
["TECHNIK","KT 68  PVC žlutá"]
["TECHNIK","KT 68 bílá"]
["TECHNIK","KT 68 černá"]
["TECHNIK","KT 68 modrá"]
["TECHNIK","KT 68 rudá"]
["TECHNIK","KT 68 žlutá"]
["TECHNIK","KTK  1"]
["TECHNIK","KTK  10/4"]
["TECHNIK","KTK  14/4"]
["TECHNIK","KTK  16/8"]
["TECHNIK","KTK  2"]
["TECHNIK","KTK  23/8"]
["TECHNIK","KTK  2T"]
["TECHNIK","KTK  33/15"]
["TECHNIK","KTK  3T"]
["TECHNIK","KTK  4"]
["TECHNIK","KTK  40/15"]
["TECHNIK","KTK  52/25"]
["TECHNIK","KTK  6"]
["TECHNIK","KTK  6H"]
["TECHNIK","KTK  70/25"]
["TECHNIK","KTK  8"]
["TECHNIK","KTK  90/45"]
["TECHNIK","KTK 11"]
["TECHNIK","KTK 120/45"]
["TECHNIK","KTK 148/57"]
["TECHNIK","KTK 160/82"]
["TECHNIK","KTK 200/90"]
["TECHNIK","KTK 68 bílá"]
["TECHNIK","KTO  1"]
["TECHNIK","KTO  2"]
["TECHNIK","KTO  2T"]
["TECHNIK","KTO  3T"]
["TECHNIK","KTO  4"]
["TECHNIK","KTO  6"]
["TECHNIK","KTO  8"]
["TECHNIK","KTO 11"]
["TECHNIK","KTU 28 PA"]
["TECHNIK","KTU 48 PA/2"]
["TECHNIK","KTU 68 PA"]
["TECHNIK","KTU 68 PA/2"]
["TECHNIK","KTU 68 PVC černá"]
["TECHNIK","KTU 68 PVC transp"]
["TECHNIK","KUR  2516"]
["TECHNIK","KUR  3525"]
["TECHNIK","KUR 12095"]
["TECHNIK","KUR 240185"]
["TECHNIK","KUR 300240"]
["TECHNIK","KUV   6-M 5"]
["TECHNIK","KUV   6-M 6"]
["TECHNIK","KUV   6-M 8"]
["TECHNIK","KUV  10-M 4"]
["TECHNIK","KUV  10-M 5"]
["TECHNIK","KUV  10-M 6"]
["TECHNIK","KUV  10-M 8"]
["TECHNIK","KUV  10-M10"]
["TECHNIK","KUV  16-M 6"]
["TECHNIK","KUV  16-M 8"]
["TECHNIK","KUV  16-M10"]
["TECHNIK","KUV  16-M12"]
["TECHNIK","KUV  25-M 6"]
["TECHNIK","KUV  25-M 8"]
["TECHNIK","KUV  25-M10"]
["TECHNIK","KUV  25-M12"]
["TECHNIK","KUV  35-M 6"]
["TECHNIK","KUV  35-M 8"]
["TECHNIK","KUV  35-M10"]
["TECHNIK","KUV  35-M12"]
["TECHNIK","KUV  35-M16"]
["TECHNIK","KUV  50-M 6"]
["TECHNIK","KUV  50-M 8"]
["TECHNIK","KUV  50-M10"]
["TECHNIK","KUV  50-M12"]
["TECHNIK","KUV  50-M16"]
["TECHNIK","KUV  70-M 8"]
["TECHNIK","KUV  70-M10"]
["TECHNIK","KUV  70-M12"]
["TECHNIK","KUV  70-M16"]
["TECHNIK","KUV  70-M20"]
["TECHNIK","KUV  95-M 8"]
["TECHNIK","KUV  95-M10"]
["TECHNIK","KUV  95-M12"]
["TECHNIK","KUV  95-M16"]
["TECHNIK","KUV 120-M10"]
["TECHNIK","KUV 120-M12"]
["TECHNIK","KUV 120-M16"]
["TECHNIK","KUV 120-M20"]
["TECHNIK","KUV 150-M10"]
["TECHNIK","KUV 150-M12"]
["TECHNIK","KUV 150-M16"]
["TECHNIK","KUV 150-M20"]
["TECHNIK","KUV 185-M10"]
["TECHNIK","KUV 185-M12"]
["TECHNIK","KUV 185-M16"]
["TECHNIK","KUV 185-M20"]
["TECHNIK","KUV 240-M10"]
["TECHNIK","KUV 240-M12"]
["TECHNIK","KUV 240-M16"]
["TECHNIK","KUV 240-M20"]
["TECHNIK","KUV 300-M12"]
["TECHNIK","KUV 300-M16"]
["TECHNIK","KUV 300-M20"]
["TECHNIK","KUV 400-M16"]
["TECHNIK","KUV 400-M20"]
["TECHNIK","KUV 500-2xM16/40"]
["TECHNIK","KUV 500-M12"]
["TECHNIK","KUV 500-M16"]
["TECHNIK","KUV 500-M20"]
["TECHNIK","KUV 625-M16"]
["TECHNIK","KUZEV  16"]
["TECHNIK","KUZEV  25"]
["TECHNIK","KUZEV  50"]
["TECHNIK","KUZEV 120"]
["TECHNIK","KUZEV 150"]
["TECHNIK","KUZEV 300"]
["TECHNIK","KUZEV 500"]
["TECHNIK","KY 2"]
["TECHNIK","KY 3"]
["TECHNIK","KY 4"]
["TECHNIK","KY 8161"]
["TECHNIK","KY175  2,4/1,2 trans"]
["TECHNIK","KY175  3,2/1,6 trans"]
["TECHNIK","KY-D 056"]
["TECHNIK","KY-D 35"]
["TECHNIK","KY-OI 056"]
["TECHNIK","KY-ON 0510"]
["TECHNIK","KY-SET"]
["TECHNIK SPECIAL - AKCIA","L  6-22"]
["TECHNIK SPECIAL - AKCIA","L  6-45"]
["TECHNIK SPECIAL - AKCIA","L  6-50"]
["TECHNIK SPECIAL - AKCIA","L 10-22"]
["TECHNIK SPECIAL - AKCIA","L 10-45"]
["TECHNIK SPECIAL - AKCIA","L 10-50"]
["TECHNIK SPECIAL - AKCIA","L 10-C"]
["TECHNIK SPECIAL - AKCIA","L 16-22"]
["TECHNIK SPECIAL - AKCIA","L 16-45"]
["TECHNIK SPECIAL - AKCIA","L 16-50"]
["TECHNIK SPECIAL - AKCIA","L 16-C"]
["TECHNIK SPECIAL - AKCIA","L 25-22"]
["TECHNIK SPECIAL - AKCIA","L 25-45"]
["TECHNIK SPECIAL - AKCIA","L 25-50"]
["TECHNIK SPECIAL - AKCIA","L 25-C"]
["TECHNIK SPECIAL - AKCIA","L 35-22"]
["TECHNIK SPECIAL - AKCIA","L 35-45"]
["TECHNIK SPECIAL - AKCIA","L 35-50"]
["TECHNIK SPECIAL - AKCIA","L 35-C"]
["TECHNIK SPECIAL - AKCIA","L 50-22"]
["TECHNIK SPECIAL - AKCIA","L 50-45"]
["TECHNIK SPECIAL - AKCIA","L 50-50"]
["TECHNIK SPECIAL - AKCIA","L 50-C"]
["TECHNIK SPECIAL - AKCIA","L 70-22"]
["TECHNIK SPECIAL - AKCIA","L 70-45"]
["TECHNIK SPECIAL - AKCIA","L 70-50"]
["TECHNIK SPECIAL - AKCIA","L 70-C"]
["TECHNIK SPECIAL - AKCIA","L 95-22"]
["TECHNIK SPECIAL - AKCIA","L 95-45"]
["TECHNIK SPECIAL - AKCIA","L 95-50"]
["TECHNIK SPECIAL - AKCIA","L 95-C"]
["TECHNIK SPECIAL - AKCIA","L120-22"]
["TECHNIK SPECIAL - AKCIA","L120-45"]
["TECHNIK SPECIAL - AKCIA","L120-50"]
["TECHNIK SPECIAL - AKCIA","L120-C"]
["TECHNIK SPECIAL - AKCIA","L130-D 10"]
["TECHNIK SPECIAL - AKCIA","L130-L 10"]
["TECHNIK SPECIAL - AKCIA","L150-22"]
["TECHNIK SPECIAL - AKCIA","L150-3D"]
["TECHNIK SPECIAL - AKCIA","L150-45"]
["TECHNIK SPECIAL - AKCIA","L150-50"]
["TECHNIK SPECIAL - AKCIA","L150-C"]
["TECHNIK SPECIAL - AKCIA","L185-22"]
["TECHNIK SPECIAL - AKCIA","L185-3D"]
["TECHNIK SPECIAL - AKCIA","L185-50"]
["TECHNIK SPECIAL - AKCIA","L185-C"]
["TECHNIK SPECIAL - AKCIA","L240-22"]
["TECHNIK SPECIAL - AKCIA","L240-3D"]
["TECHNIK SPECIAL - AKCIA","L240-50"]
["TECHNIK SPECIAL - AKCIA","L240-C"]
["TECHNIK SPECIAL - AKCIA","L300-19"]
["TECHNIK SPECIAL - AKCIA","L300-22"]
["TECHNIK SPECIAL - AKCIA","L300-3D"]
["TECHNIK SPECIAL - AKCIA","L300-C"]
["TECHNIK SPECIAL - AKCIA","L400-3D"]
["TECHNIK SPECIAL - AKCIA","L400-C"]
["TECHNIK SPECIAL - AKCIA","L500-3D"]
["TECHNIK SPECIAL - AKCIA","L625-3D"]
["TECHNIK","LB-SET 10"]
["TECHNIK","LB-SET 5"]
["TECHNIK SPECIAL - AKCIA","LC 100"]
["TECHNIK","LD 0,14-2,5"]
["TECHNIK","LD 0,25-6"]
["TECHNIK","LDR 0256"]
["TECHNIK","LDR 1025"]
["TECHNIK","LDZ 6-16"]
["TECHNIK","Lepidlo ve spreji"]
["TECHNIK","LetraTag MOMENTUM"]
["TECHNIK","LetraTag RAZOR"]
["TECHNIK","LFC2-4,8x200"]
["TECHNIK","LF-SET"]
["TECHNIK SPECIAL - AKCIA","LH 130"]
["TECHNIK SPECIAL - AKCIA","LH 130K"]
["TECHNIK","LH-SET"]
["TECHNIK","LI 0,08-1,5"]
["TECHNIK","LI 0,25-2,5"]
["TECHNIK","LIR 056"]
["TECHNIK","LK  2/Z"]
["TECHNIK","LK 0,1-1"]
["TECHNIK","LK 0,14-1,5"]
["TECHNIK","LK 0,5-2,5"]
["TECHNIK","LK-0525 BP"]
["TECHNIK","LK-0525 BP/P"]
["TECHNIK","LK1"]
["TECHNIK","LK1 CHROM"]
["TECHNIK","LK1-BP 051"]
["TECHNIK","LK1-BP 1525"]
["TECHNIK","LK1-D0256"]
["TECHNIK","LK1-D1025"]
["TECHNIK","LK1-D3550"]
["TECHNIK","LK1-D70"]
["TECHNIK","LK1-D95"]
["TECHNIK","LK1-DSK 08056"]
["TECHNIK","LK1-DSK 08056 LOC"]
["TECHNIK","LK1-H&S 4"]
["TECHNIK","LK1-H&S 6"]
["TECHNIK","LK1-HIR"]
["TECHNIK","LK1-KK 01415"]
["TECHNIK","LK1-KOAX"]
["TECHNIK","LK1-MC 3"]
["TECHNIK","LK1-MC 3 LOC"]
["TECHNIK","LK1-MC 4"]
["TECHNIK","LK1-MC 4 LOC"]
["TECHNIK","LK1-MC 4/4 UNI"]
["TECHNIK","LK1-MC 4/6 UNI"]
["TECHNIK","LK1-MK 0525"]
["TECHNIK","LK1-MO 0125"]
["TECHNIK","LK1-MO 0125 LOC"]
["TECHNIK","LK1-MO 056"]
["TECHNIK","LK1-MO 056 LOC"]
["TECHNIK","LK1-MOJ 056 LOC"]
["TECHNIK","LK1-OI 056"]
["TECHNIK","LK1-OI 1016"]
["TECHNIK","LK1-OL 1510"]
["TECHNIK","LK1-ON 02525"]
["TECHNIK","LK1-ON 0510"]
["TECHNIK","LK1-ON 1625"]
["TECHNIK","LK1-SIS 056"]
["TECHNIK","LK1-SK 0144"]
["TECHNIK","LK1-SK 0144 LOC"]
["TECHNIK","LK1-SK 156"]
["TECHNIK","LK1-SK 156 LOC"]
["TECHNIK","LK1-SK 410"]
["TECHNIK","LK1-SK 410 LOC"]
["TECHNIK","LK1-SK 625 LOC"]
["TECHNIK","LK1-SK1016 LOC"]
["TECHNIK","LK1-T/TM11"]
["TECHNIK","LK1-TYCO"]
["TECHNIK","LK1-TYCO/LOC"]
["TECHNIK","LK-2"]
["TECHNIK","LK-2KY"]
["TECHNIK","LK-2P"]
["TECHNIK","LK-2TF"]
["TECHNIK","LK-2TF PLUS"]
["TECHNIK","LK-2Z"]
["TECHNIK","LK-3"]
["TECHNIK SPECIAL - AKCIA","LK330"]
["TECHNIK SPECIAL - AKCIA","LK330 nůž"]
["TECHNIK","LK330 PÁS 6 bílá"]
["TECHNIK","LK330 PÁS 6 stříbrná"]
["TECHNIK","LK330 PÁS 6 žlutá"]
["TECHNIK","LK330 PÁS 9 bílá"]
["TECHNIK","LK330 PÁS 9 stříbrná"]
["TECHNIK","LK330 PÁS 9 žlutá"]
["TECHNIK","LK330 PÁS12 bílá"]
["TECHNIK","LK330 PÁS12 stříbrná"]
["TECHNIK","LK330 PÁS12 žlutá"]
["TECHNIK","LK330 TISK černá"]
["TECHNIK","LK-CC"]
["TECHNIK","LK-CC/0"]
["TECHNIK","LK-D 02516"]
["TECHNIK","LK-D 02516 P"]
["TECHNIK","LK-D 02516/1000"]
["TECHNIK","LK-D 02525"]
["TECHNIK","LK-D 02525/2"]
["TECHNIK","LK-D 0256"]
["TECHNIK","LK-D 0256U6"]
["TECHNIK","LK-D 0516"]
["TECHNIK","LK-D 0516/2"]
["TECHNIK","LK-D 0525"]
["TECHNIK","LK-D 0525 P"]
["TECHNIK","LK-D 0525 P/1000"]
["TECHNIK","LK-D 054"]
["TECHNIK","LK-D 056"]
["TECHNIK","LK-D 07510"]
["TECHNIK","LK-D 0810"]
["TECHNIK","LK-D 1035"]
["TECHNIK","LK-D 1050"]
["TECHNIK","LK-D 1050 E"]
["TECHNIK","LK-D 120150 E"]
["TECHNIK","LK-D 156"]
["TECHNIK","LK-D 1650"]
["TECHNIK","LK-D 2516"]
["TECHNIK","LK-D 416"]
["TECHNIK","LK-D 5095"]
["TECHNIK","LK-D 5095 E"]
["TECHNIK","LK-D 6"]
["TECHNIK","LK-D 616"]
["TECHNIK","LK-DSK 05075"]
["TECHNIK","LK-DSK 05075/P"]
["TECHNIK","LK-DSK 0805"]
["TECHNIK","LK-DSK 0805/P"]
["TECHNIK","LK-D-SUB"]
["TECHNIK SPECIAL - AKCIA","LKE1"]
["TECHNIK","LK-KK 02515"]
["TECHNIK","LK-KK 02515/P"]
["TECHNIK","LKM 6/70"]
["TECHNIK","LKM 6/70 D"]
["TECHNIK","LK-MC 3"]
["TECHNIK","LK-MC 3/P"]
["TECHNIK","LK-MC 4"]
["TECHNIK","LK-MC 4/P"]
["TECHNIK","LK-MC 4/TF"]
["TECHNIK","LK-MO 0221"]
["TECHNIK","LK-MO 051 BP-A"]
["TECHNIK","LK-MO 051 BP-A/P"]
["TECHNIK","LK-MO 0525"]
["TECHNIK","LK-MO 0525 BP/P"]
["TECHNIK","LK-MO 0525 BP-B"]
["TECHNIK","LK-MO 0525 BP-B/P"]
["TECHNIK","LK-MO 056"]
["TECHNIK","LK-MO 1525 BP-A"]
["TECHNIK","LK-MO 1525 BP-A/P"]
["TECHNIK","LK-OI 056"]
["TECHNIK","LK-OL 056"]
["TECHNIK","LK-OL 056/P"]
["TECHNIK","LK-OL 07516"]
["TECHNIK","LK-ON 0510"]
["TECHNIK","LK-ON 0516"]
["TECHNIK","LKR 0125"]
["TECHNIK","LKR 056"]
["TECHNIK","LKS 0,03-0,56"]
["TECHNIK","LKS 0,08-1,3"]
["TECHNIK","LKS 0,08-2,5"]
["TECHNIK","LKS 0,14-3,3"]
["TECHNIK","LK-SIS 056"]
["TECHNIK","LK-SIS 056/P"]
["TECHNIK","LK-SIS 056/TF"]
["TECHNIK","LK-SK 01405"]
["TECHNIK","LK-SK 054"]
["TECHNIK","LK-T  4"]
["TECHNIK","LK-T  6"]
["TECHNIK","LK-T  8"]
["TECHNIK","LK-T  8/TF"]
["TECHNIK","LK-T 10"]
["TECHNIK","LK-T 10/E"]
["TECHNIK","LK-T 10/P"]
["TECHNIK","LK-T 46"]
["TECHNIK","LK-T 68"]
["TECHNIK","LK-T 68 P"]
["TECHNIK","LKT1"]
["TECHNIK","LK-T4610"]
["TECHNIK","LK-T468"]
["TECHNIK","LK-T468 A"]
["TECHNIK","LK-T468 H"]
["TECHNIK","LK-T468 P"]
["TECHNIK","LK-X1"]
["TECHNIK","LK-X2"]
["TECHNIK","LK-X3"]
["TECHNIK","LK-X4"]
["TECHNIK","LK-X5"]
["TECHNIK","LK-X6"]
["TECHNIK","LK-X7"]
["TECHNIK","LKZ-0525 BP"]
["TECHNIK","LKZ-D 054"]
["TECHNIK","LKZ-D 056"]
["TECHNIK","LKZ-D 056/OI 0525"]
["TECHNIK","LKZ-D 1025"]
["TECHNIK","LKZ-D 1035"]
["TECHNIK","LKZ-D 110"]
["TECHNIK","LKZ-D 2550"]
["TECHNIK","LKZ-D 616"]
["TECHNIK","LKZ-MO 011"]
["TECHNIK","LKZ-MO 01425"]
["TECHNIK","LKZ-MO 0256"]
["TECHNIK","LKZ-MO 051 BP-A"]
["TECHNIK","LKZ-MO 0525 BP-B"]
["TECHNIK","LKZ-MO 056"]
["TECHNIK","LKZ-MO 1525 BP-A"]
["TECHNIK","LKZ-OI 0146"]
["TECHNIK","LKZ-OI 056"]
["TECHNIK","LKZ-OI 1016"]
["TECHNIK","LKZ-ON 0510"]
["TECHNIK","LKZ-ON 2516"]
["TECHNIK","LKZ-SK 156"]
["TECHNIK","LM 160"]
["TECHNIK","LM 160+3"]
["TECHNIK","LM 210D"]
["TECHNIK","LM 280"]
["TECHNIK","LM 280+4"]
["TECHNIK","LM 360D"]
["TECHNIK","LM 420P"]
["TECHNIK","LM 500TS"]
["TECHNIK","LM PnP AKCE"]
["TECHNIK","LM PnP wireless"]
["TECHNIK","LM PnP+2"]
["TECHNIK","LN 0,25-2,5"]
["TECHNIK","LN 1,5-6"]
["TECHNIK","LNR 02525"]
["TECHNIK","LNR 0510"]
["TECHNIK","LOC1-DSK 08056"]
["TECHNIK","LOC1-MC 3"]
["TECHNIK","LOC1-MC 4"]
["TECHNIK","LOC1-MO 056"]
["TECHNIK","LOC1-MOJ 056"]
["TECHNIK","LOC1-SK 0144"]
["TECHNIK","LOC1-TYCO"]
["TECHNIK","LOC-LS 0,14-6"]
["REIKU-B","LPRRB-10F"]
["REIKU-B","LPRRB-12F"]
["REIKU-B","LPRRB-17F"]
["REIKU-B","LPRRB-23G"]
["REIKU-B","LPRRB-29G"]
["REIKU-B","LPRRB-36G"]
["REIKU-B","LPRRB-48G"]
["REIKU-B","LPRRB-52G"]
["REIKU-B","LPRRB-70G"]
["REIKU-B","LPRRB-95G"]
["TECHNIK SPECIAL - AKCIA","LPV 120/12"]
["TECHNIK","LR 25 T"]
["TECHNIK","LR 28"]
["TECHNIK","LR 45"]
["TECHNIK","LR 48"]
["TECHNIK","LR 68 A"]
["TECHNIK","LR 68 K"]
["TECHNIK","LR SET 5"]
["TECHNIK","LRC 25 T"]
["TECHNIK","LRC 28"]
["TECHNIK","LRC 28 T"]
["TECHNIK","LRC 45"]
["TECHNIK","LRC 48"]
["TECHNIK","LRC 68 A"]
["TECHNIK","LRC 68 K"]
["TECHNIK","LS  0,5"]
["TECHNIK","LS  0,5 / 100"]
["TECHNIK","LS  1,5"]
["TECHNIK","LS  1,5 / 100"]
["TECHNIK","LS  2,5"]
["TECHNIK","LS  2,5 / 100"]
["TECHNIK","LS  6"]
["TECHNIK","LS  6 / 100"]
["TECHNIK","LS 0,08-2,5"]
["TECHNIK","LS 0,08-2,5 LOC"]
["TECHNIK","LS 0,14-6"]
["TECHNIK","LS 0,14-6 LOC"]
["TECHNIK","LS 1,5-10"]
["TECHNIK","LS 10"]
["TECHNIK","LS CWT-3809"]
["TECHNIK SPECIAL - AKCIA","LS6 Pg9-21"]
["TECHNIK","LSD  0,5"]
["TECHNIK","LSD  1,5"]
["TECHNIK","LSD  2,5"]
["TECHNIK","LSD  6"]
["TECHNIK","LSD-SET"]
["TECHNIK","LSR 1510"]
["TECHNIK","LS-SET"]
["TECHNIK","LS-SET-H"]
["TECHNIK","LU 28"]
["TECHNIK","LU 68"]
["TECHNIK","LUC 28"]
["TECHNIK","LUC 68"]
["TECHNIK","LW 450"]
["TECHNIK","LW 450 Duo"]
["TECHNIK","LW 450 Turbo"]
["TECHNIK","LW 450 Twin"]
["TECHNIK","LW 4XL"]
["TECHNIK","LXR 1"]
["TECHNIK","LZ-SET"]
["TECHNIK","M 42"]
["TECHNIK","M 42 A"]
["TECHNIK","M 42 P"]
["TECHNIK SPECIAL - AKCIA","M ovál 13,5x20"]
["TECHNIK","M. 16-95"]
["TECHNIK","M. 50-150"]
["TECHNIK","M. 95-240"]
["TECHNIK","M.120-300"]
["TECHNIK","M.185-400"]
["TECHNIK SPECIAL - AKCIA","M-1  Pro IV + kufr"]
["TECHNIK SPECIAL - AKCIA","M-1  Std III + kufr"]
["TECHNIK SPECIAL - AKCIA","M-1 adaptér 230V"]
["TECHNIK SPECIAL - AKCIA","M-1 čistící sada"]
["TECHNIK SPECIAL - AKCIA","M-1 čistící sada 2"]
["TECHNIK SPECIAL - AKCIA","M-1 čistící sada 3"]
["TECHNIK SPECIAL - AKCIA","M-1 deska OBM"]
["TECHNIK SPECIAL - AKCIA","M-1 kufr AL"]
["TECHNIK SPECIAL - AKCIA","M-1 navádění"]
["TECHNIK SPECIAL - AKCIA","M-1 navádění 2"]
["TECHNIK","M-1 NN  6 bílá"]
["TECHNIK","M-1 NN  6 stříbrná"]
["TECHNIK","M-1 NN  6 žlutá"]
["TECHNIK","M-1 NN  9 bílá"]
["TECHNIK","M-1 NN  9 stříbrná"]
["TECHNIK","M-1 NN  9 žlutá"]
["TECHNIK","M-1 NN 12 bílá"]
["TECHNIK","M-1 NN 12 stříbrná"]
["TECHNIK","M-1 NN 12 žlutá"]
["TECHNIK SPECIAL - AKCIA","M-1 nůž"]
["TECHNIK","M-1 OBM-PÁSKA"]
["TECHNIK","M-1 OBM-PÁSKA 33"]
["TECHNIK SPECIAL - AKCIA","M-1 odvíjení"]
["TECHNIK","M-1 PÁSEK  4 bílá"]
["TECHNIK","M-1 PÁSEK  4 žlutá"]
["TECHNIK","M-1 PÁSEK  9 bílá"]
["TECHNIK","M-1 PÁSEK  9 žlutá"]
["TECHNIK","M-1 PÁSEK 12 bílá"]
["TECHNIK","M-1 PÁSEK 12 žlutá"]
["TECHNIK","M-1 PÁSKA  6 bílá"]
["TECHNIK","M-1 PÁSKA  6 stříbr."]
["TECHNIK","M-1 PÁSKA  6 žlutá"]
["TECHNIK","M-1 PÁSKA  9 bílá"]
["TECHNIK","M-1 PÁSKA  9 stříbr."]
["TECHNIK","M-1 PÁSKA  9 žlutá"]
["TECHNIK","M-1 PÁSKA 12 bílá"]
["TECHNIK","M-1 PÁSKA 12 stříbr."]
["TECHNIK","M-1 PÁSKA 12 žlutá"]
["TECHNIK SPECIAL - AKCIA","M-1 podávání"]
["TECHNIK SPECIAL - AKCIA","M-1 předehřívání"]
["TECHNIK","M-1 SB bílá 3,2/1,6"]
["TECHNIK","M-1 SB bílá 3/1"]
["TECHNIK","M-1 SB bílá 4,8/2,4"]
["TECHNIK","M-1 SB bílá 6,4/3,2"]
["TECHNIK","M-1 SB bílá 6/2"]
["TECHNIK","M-1 SB žlutá 3,2/1,6"]
["TECHNIK","M-1 SB žlutá 3/1"]
["TECHNIK","M-1 SB žlutá 4,8/2,4"]
["TECHNIK","M-1 SB žlutá 6,4/3,2"]
["TECHNIK","M-1 SB žlutá 6/2"]
["TECHNIK","M-1/CH TISK bílá"]
["TECHNIK","M-1/CH TISK bílá ID"]
["TECHNIK","M-1/CH TISK černá ID"]
["TECHNIK","M-1/CH TISK černá MS"]
["TECHNIK SPECIAL - AKCIA","M-3E"]
["TECHNIK","M-3E páska 30mm Č"]
["TECHNIK","M-3E páska 35mm Č"]
["TECHNIK SPECIAL - AKCIA","M-3E razník"]
["TECHNIK SPECIAL - AKCIA","MA  2-C"]
["TECHNIK SPECIAL - AKCIA","MA  3-C"]
["TECHNIK SPECIAL - AKCIA","MA  5-C"]
["TECHNIK SPECIAL - AKCIA","MA  7-C"]
["TECHNIK SPECIAL - AKCIA","MA 10-C"]
["TECHNIK SPECIAL - AKCIA","MA 14-C"]
["TECHNIK SPECIAL - AKCIA","MA 19-C"]
["TECHNIK SPECIAL - AKCIA","MA 24-C"]
["TECHNIK SPECIAL - AKCIA","MA 30-C"]
["TECHNIK SPECIAL - AKCIA","MA 37-C"]
["TECHNIK SPECIAL - AKCIA","MA 48-C"]
["TECHNIK SPECIAL - AKCIA","MA 60-C"]
["TECHNIK SPECIAL - AKCIA","MATRICE L  6,6"]
["TECHNIK SPECIAL - AKCIA","MATRICE L  9,0"]
["TECHNIK SPECIAL - AKCIA","MATRICE L  9,5"]
["TECHNIK SPECIAL - AKCIA","MATRICE L 11,0"]
["TECHNIK SPECIAL - AKCIA","MATRICE L 13,5"]
["TECHNIK SPECIAL - AKCIA","MATRICE L 17,5"]
["TECHNIK SPECIAL - AKCIA","MATRICE L 21,5"]
["TECHNIK SPECIAL - AKCIA","MATRICE S  9,0"]
["TECHNIK SPECIAL - AKCIA","MATRICE S 11,0"]
["TECHNIK SPECIAL - AKCIA","MATRICE S 13,5"]
["TECHNIK SPECIAL - AKCIA","MATRICE S 6,6"]
["TECHNIK SPECIAL - AKCIA","MC  40L"]
["TECHNIK SPECIAL - AKCIA","MC  40L/ 4"]
["TECHNIK SPECIAL - AKCIA","MC  40L/ 6"]
["TECHNIK SPECIAL - AKCIA","MC  40L/10"]
["TECHNIK SPECIAL - AKCIA","MC 25"]
["TECHNIK SPECIAL - AKCIA","MC 40"]
["TECHNIK SPECIAL - AKCIA","MC 40/258"]
["TECHNIK SPECIAL - AKCIA","MC 40/346"]
["TECHNIK SPECIAL - AKCIA","MC 40/348"]
["TECHNIK SPECIAL - AKCIA","MC 40/410"]
["TECHNIK SPECIAL - AKCIA","MC 40/L 6"]
["TECHNIK SPECIAL - AKCIA","MC 40/L10"]
["TECHNIK SPECIAL - AKCIA","MC 40/L12"]
["TECHNIK SPECIAL - AKCIA","MC2 0100"]
["TECHNIK","MD 02"]
["TECHNIK","MD 02/3 euro 0-9"]
["TECHNIK","MD 02/3 žlutá 0-9"]
["TECHNIK","MD 02/3.4"]
["TECHNIK","MD 02/3.40\"-\""]
["TECHNIK","MD 02/3.40\"+\""]
["TECHNIK","MD 02/3.40\"0\""]
["TECHNIK","MD 02/3.40\"1\""]
["TECHNIK","MD 02/3.40\"2\""]
["TECHNIK","MD 02/3.40\"3\""]
["TECHNIK","MD 02/3.40\"4\""]
["TECHNIK","MD 02/3.40\"5\""]
["TECHNIK","MD 02/3.40\"6\""]
["TECHNIK","MD 02/3.40\"7\""]
["TECHNIK","MD 02/3.40\"8\""]
["TECHNIK","MD 02/3.40\"9\""]
["TECHNIK","MD 02/3.40\"A\""]
["TECHNIK","MD 02/3.40\"B\""]
["TECHNIK","MD 02/3.40\"C\""]
["TECHNIK","MD 02/3.40\"E\""]
["TECHNIK","MD 02/3.40\"U\""]
["TECHNIK","MD 02/3.40\"V\""]
["TECHNIK","MD 02/3.40\"W\""]
["TECHNIK","MD 10"]
["TECHNIK","MD 10/3 žlutá 0-9"]
["TECHNIK","MD 10/3.4"]
["TECHNIK","MD 10/3.40\"-\""]
["TECHNIK","MD 10/3.40\"+\""]
["TECHNIK","MD 10/3.40\"0\""]
["TECHNIK","MD 10/3.40\"1\""]
["TECHNIK","MD 10/3.40\"2\""]
["TECHNIK","MD 10/3.40\"3\""]
["TECHNIK","MD 10/3.40\"4\""]
["TECHNIK","MD 10/3.40\"5\""]
["TECHNIK","MD 10/3.40\"6\""]
["TECHNIK","MD 10/3.40\"7\""]
["TECHNIK","MD 10/3.40\"8\""]
["TECHNIK","MD 10/3.40\"9\""]
["TECHNIK","MD 10/3.40\"A\""]
["TECHNIK","MD 10/3.40\"C\""]
["TECHNIK","MD 10/3.40\"G\""]
["TECHNIK","MD 10/3.40\"H\""]
["TECHNIK","MD 10/3.40\"L\""]
["TECHNIK","MD 10/3.40\"N\""]
["TECHNIK","MD 10/3.40\"R\""]
["TECHNIK","MD 10/3.40\"S\""]
["TECHNIK","MD 10/3.40\"U\""]
["TECHNIK","MD 10/3.40\"V\""]
["TECHNIK","MD 10/3.40\"W\""]
["TECHNIK","MD 10/6.40\"PE\""]
["TECHNIK","MDH 2002"]
["TECHNIK","MDH 2002 K"]
["TECHNIK","MDH 2010"]
["TECHNIK","MDH 2010 K"]
["TECHNIK","Měď sprej"]
["REIKU-B","MES1B-07"]
["REIKU-B","MES1B-10"]
["REIKU-B","MES1B-12"]
["REIKU-B","MES1B-14"]
["REIKU-B","MES1B-17"]
["REIKU-B","MES1B-23"]
["REIKU-B","MES1B-29"]
["REIKU-B","MES1B-36"]
["REIKU-B","MES1B-48"]
["REIKU-B","MES1B-52"]
["REIKU-B","MES1B-70"]
["REIKU-B","MES2B-52"]
["REIKU-B","MES2B-70"]
["REIKU-B","MES2B-95"]
["TECHNIK","Metal Fluid sprej"]
["TECHNIK","MG9"]
["TECHNIK","MHP  6/50"]
["TECHNIK","MHP  6/50 D"]
["TECHNIK","MHP 10/120"]
["TECHNIK","MHP 10/120 D"]
["TECHNIK","MHP 16/95"]
["TECHNIK","MHP 16/95 D"]
["TECHNIK","MHP 25/150"]
["TECHNIK","MHP 25/150 D"]
["TECHNIK","MHPL  6/50"]
["TECHNIK","MHPL  6/50 D"]
["TECHNIK","MHPL 10/120"]
["TECHNIK","MHPL 10/120 D"]
["TECHNIK","MHPL 25/150"]
["TECHNIK","MHPL 25/150 D"]
["TECHNIK","MHPL 70/240 D"]
["TECHNIK","MK 1,5-25"]
["TECHNIK","MK 1,5-28"]
["TECHNIK","MK 1,5-45"]
["TECHNIK","MK 1,5-48"]
["TECHNIK","MK 1,5-68"]
["TECHNIK","MK 1,5-68 P"]
["TECHNIK","MK 2,5-68"]
["TECHNIK","MK 2,5-68 K"]
["TECHNIK","MK 2,5-68 P"]
["TECHNIK","MK 6-68"]
["TECHNIK","MK 6-68 P"]
["TECHNIK","MKC 1,5-25"]
["TECHNIK","MKC 1,5-28"]
["TECHNIK","MKC 1,5-45"]
["TECHNIK","MKC 1,5-48"]
["TECHNIK","MKC 1,5-68"]
["TECHNIK","MKC 1,5-68 P"]
["TECHNIK","MKC 2,5-68 "]
["TECHNIK","MKC 2,5-68 K"]
["TECHNIK","MKC 2,5-68 P"]
["TECHNIK","MKC 6-68"]
["TECHNIK","MKC 6-68 P"]
["TECHNIK","MKJ 1,5-25"]
["TECHNIK","MKJ 1,5-28"]
["TECHNIK","MKJ 1,5-68"]
["TECHNIK","MKJ 2,5-55"]
["TECHNIK","MKJ 2,5-68"]
["TECHNIK","MKJ 2,5-68 P"]
["TECHNIK","MKJ 6-68"]
["TECHNIK","MKJC 1,5-25"]
["TECHNIK","MKJC 1,5-28"]
["TECHNIK","MKJC 1,5-48"]
["TECHNIK","MKJC 1,5-68"]
["TECHNIK","MKJC 1,5-68 P"]
["TECHNIK","MKJC 2,5-68"]
["TECHNIK","MKJC 2,5-68 P"]
["TECHNIK","MKJC 6-68"]
["TECHNIK","MKJC 6-68 P"]
["TECHNIK","MM 1"]
["TECHNIK","MM 1-1"]
["TECHNIK","MM 1-2"]
["TECHNIK","MM 1-3"]
["TECHNIK","MM 2"]
["TECHNIK","MM 3"]
["TECHNIK","MM 4"]
["TECHNIK","MM 7-1"]
["TECHNIK","MM 9"]
["TECHNIK","MM P3"]
["TECHNIK","MM10"]
["TECHNIK","MM11"]
["TECHNIK","MO 0,25-25"]
["TECHNIK","MO 0,25-28"]
["TECHNIK","MO 0,5-25"]
["TECHNIK","MO 0,5-28"]
["TECHNIK","MO 1,5-25"]
["TECHNIK","MO 1,5-25 K"]
["TECHNIK","MO 1,5-28"]
["TECHNIK","MO 1,5-28 K"]
["TECHNIK","MO 1,5-45"]
["TECHNIK","MO 1,5-45 P"]
["TECHNIK","MO 1,5-48"]
["TECHNIK","MO 1,5-48 BP"]
["TECHNIK","MO 1,5-48 BP-B"]
["TECHNIK","MO 1,5-48 P"]
["TECHNIK","MO 1,5-68"]
["TECHNIK","MO 1,5-68 BP"]
["TECHNIK","MO 1,5-68 BP-B"]
["TECHNIK","MO 1,5-68 P"]
["TECHNIK SPECIAL - AKCIA","MO 16-22"]
["TECHNIK SPECIAL - AKCIA","MO 18-22"]
["TECHNIK","MO 2,5-45"]
["TECHNIK","MO 2,5-48"]
["TECHNIK","MO 2,5-68"]
["TECHNIK","MO 2,5-68 BP"]
["TECHNIK","MO 2,5-68 BP-B"]
["TECHNIK","MO 2,5-68 P"]
["TECHNIK","MO 6-68"]
["TECHNIK","MO 6-68 P"]
["TECHNIK","MO 6-91"]
["TECHNIK SPECIAL - AKCIA","MO.12-22"]
["TECHNIK SPECIAL - AKCIA","MO.20-22"]
["TECHNIK SPECIAL - AKCIA","MO.22-22"]
["TECHNIK SPECIAL - AKCIA","MO.24-22"]
["TECHNIK SPECIAL - AKCIA","MO.26-22"]
["TECHNIK","MOC 0,25-25"]
["TECHNIK","MOC 0,25-28"]
["TECHNIK","MOC 0,5-25"]
["TECHNIK","MOC 0,5-28"]
["TECHNIK","MOC 1,0-28"]
["TECHNIK","MOC 1,5-25"]
["TECHNIK","MOC 1,5-25 K"]
["TECHNIK","MOC 1,5-28"]
["TECHNIK","MOC 1,5-28 K"]
["TECHNIK","MOC 1,5-45"]
["TECHNIK","MOC 1,5-45 P"]
["TECHNIK","MOC 1,5-48"]
["TECHNIK","MOC 1,5-48 BP"]
["TECHNIK","MOC 1,5-48 BP-B"]
["TECHNIK","MOC 1,5-48 P"]
["TECHNIK","MOC 1,5-48/IMP"]
["TECHNIK","MOC 1,5-68"]
["TECHNIK","MOC 1,5-68 BP"]
["TECHNIK","MOC 1,5-68 BP-B"]
["TECHNIK","MOC 1,5-68 BP-B P"]
["TECHNIK","MOC 1,5-68 J"]
["TECHNIK","MOC 1,5-68 MX"]
["TECHNIK","MOC 1,5-68 P"]
["TECHNIK","MOC 2,5-45"]
["TECHNIK","MOC 2,5-48"]
["TECHNIK","MOC 2,5-68"]
["TECHNIK","MOC 2,5-68 BP"]
["TECHNIK","MOC 2,5-68 BP MX"]
["TECHNIK","MOC 2,5-68 BP-B"]
["TECHNIK","MOC 2,5-68 P"]
["TECHNIK","MOC 3900-0039"]
["TECHNIK","MOC 6-68"]
["TECHNIK","MOC 6-68 P"]
["TECHNIK","MOC 6-91"]
["TECHNIK","MOJ 1,5-25"]
["TECHNIK","MOJ 1,5-28"]
["TECHNIK","MOJ 1,5-48"]
["TECHNIK","MOJ 1,5-68"]
["TECHNIK","MOJ 1,5-68 P"]
["TECHNIK","MOJ 2,5-48"]
["TECHNIK","MOJ 2,5-55"]
["TECHNIK","MOJ 2,5-68"]
["TECHNIK","MOJ 2,5-68 P"]
["TECHNIK","MOJ 2,5-88 BP"]
["TECHNIK","MOJ 6-68"]
["TECHNIK","MOJ 6-68 P"]
["TECHNIK","MOJC 1,5-25"]
["TECHNIK","MOJC 1,5-28"]
["TECHNIK","MOJC 1,5-48"]
["TECHNIK","MOJC 1,5-68"]
["TECHNIK","MOJC 1,5-68 BP"]
["TECHNIK","MOJC 1,5-68 P"]
["TECHNIK","MOJC 2,5-48"]
["TECHNIK","MOJC 2,5-68"]
["TECHNIK","MOJC 2,5-68 P"]
["TECHNIK","MOJC 6-68"]
["TECHNIK","MOJC 6-68 P"]
["TECHNIK","MOLC 68"]
["TECHNIK","MOO 1,5-48"]
["TECHNIK","MOO 1,5-68"]
["TECHNIK","MOO 1,5-68 P"]
["TECHNIK","MOO 2,5-48"]
["TECHNIK","MOO 2,5-68"]
["TECHNIK","MOO 2,5-68 P"]
["TECHNIK","MOOC 1,5-48"]
["TECHNIK","MOOC 1,5-68"]
["TECHNIK","MOOC 1,5-68 P"]
["TECHNIK","MOOC 2,5-48"]
["TECHNIK","MOOC 2,5-68"]
["TECHNIK","MOOC 2,5-68 P"]
["TECHNIK","Mosaz sprej"]
["TECHNIK SPECIAL - AKCIA","MS 24"]
["REIKU-B","MSGMM-M12"]
["REIKU-B","MSGMM-M16"]
["REIKU-B","MSGMM-M20"]
["REIKU-B","MSGMM-M25"]
["REIKU-B","MSGMM-M32"]
["REIKU-B","MSGMM-M40"]
["REIKU-B","MSGMM-M50"]
["REIKU-B","MSGMM-M63"]
["REIKU-B","MSGMM-P07"]
["REIKU-B","MSGMM-P09"]
["REIKU-B","MSGMM-P11"]
["REIKU-B","MSGMM-P13"]
["REIKU-B","MSGMM-P16"]
["REIKU-B","MSGMM-P21"]
["REIKU-B","MSGMM-P29"]
["REIKU-B","MSGMM-P36"]
["REIKU-B","MSGMM-P48"]
["REIKU-B","MSGRM-10M16 /price upon enquiry/"]
["REIKU-B","MSGRM-12M20 /price upon enquiry/"]
["REIKU-B","MSGRM-17M25 /price upon enquiry/"]
["REIKU-B","MSGRM-23M32 /price upon enquiry/"]
["REIKU-B","MSGRM-29M40 /price upon enquiry/"]
["REIKU-B","MSGRM-36M50 /price upon enquiry/"]
["REIKU-B","MSGRM-48M63 /price upon enquiry/"]
["REIKU-B","MSGVM-10M16 /price upon enquiry/"]
["REIKU-B","MSGVM-12M20 /price upon enquiry/"]
["REIKU-B","MSGVM-17M25 /price upon enquiry/"]
["REIKU-B","MSGVM-23M32 /price upon enquiry/"]
["REIKU-B","MSGVM-29M40 /price upon enquiry/"]
["REIKU-B","MSGVM-36M50 /price upon enquiry/"]
["REIKU-B","MSGVM-48M63 /price upon enquiry/"]
["TECHNIK SPECIAL - AKCIA","MSK 28"]
["REIKU-B","MSKOM-M12"]
["REIKU-B","MSKOM-M16"]
["REIKU-B","MSKOM-M20"]
["REIKU-B","MSKOM-M25"]
["REIKU-B","MSKOM-M32"]
["REIKU-B","MSKOM-M40"]
["REIKU-B","MSKOM-M50"]
["REIKU-B","MSKOM-M63"]
["REIKU-B","MSKOM-P07"]
["REIKU-B","MSKOM-P09"]
["REIKU-B","MSKOM-P11"]
["REIKU-B","MSKOM-P13"]
["REIKU-B","MSKOM-P16"]
["REIKU-B","MSKOM-P21"]
["REIKU-B","MSKOM-P29"]
["REIKU-B","MSKOM-P36"]
["REIKU-B","MSKOM-P48"]
["REIKU-B","MSM 1216"]
["REIKU-B","MSM 1612"]
["REIKU-B","MSM 1620"]
["REIKU-B","MSM 2012"]
["REIKU-B","MSM 2016"]
["REIKU-B","MSM 2025"]
["REIKU-B","MSM 2516"]
["REIKU-B","MSM 2520"]
["REIKU-B","MSM 2532"]
["REIKU-B","MSM 3220"]
["REIKU-B","MSM 3225"]
["REIKU-B","MSM 3240"]
["REIKU-B","MSM 4025"]
["REIKU-B","MSM 4032"]
["REIKU-B","MSM 4050"]
["REIKU-B","MSM 5032"]
["REIKU-B","MSM 5040"]
["REIKU-B","MSM 5063"]
["REIKU-B","MSM 6340"]
["REIKU-B","MSM 6350"]
["REIKU-B","MSP0709"]
["REIKU-B","MSP0907"]
["REIKU-B","MSP0911"]
["REIKU-B","MSP0913"]
["REIKU-B","MSP1107"]
["REIKU-B","MSP1109"]
["REIKU-B","MSP1113"]
["REIKU-B","MSP1116"]
["REIKU-B","MSP1121"]
["REIKU-B","MSP1307"]
["REIKU-B","MSP1309"]
["REIKU-B","MSP1311"]
["REIKU-B","MSP1316"]
["REIKU-B","MSP1321"]
["REIKU-B","MSP1607"]
["REIKU-B","MSP1609"]
["REIKU-B","MSP1611"]
["REIKU-B","MSP1613"]
["REIKU-B","MSP1621"]
["REIKU-B","MSP1629"]
["REIKU-B","MSP2111"]
["REIKU-B","MSP2113"]
["REIKU-B","MSP2116"]
["REIKU-B","MSP2129"]
["REIKU-B","MSP2916"]
["REIKU-B","MSP2921"]
["REIKU-B","MSP2936"]
["REIKU-B","MSP3621"]
["REIKU-B","MSP3629"]
["REIKU-B","MSP4229"]
["REIKU-B","MSP4236"]
["REIKU-B","MSP4248"]
["REIKU-B","MSP4836"]
["REIKU-B","MSP4842"]
["REIKU-B","MSPAM-M16"]
["REIKU-B","MSPAM-M20"]
["REIKU-B","MSPAM-M25"]
["REIKU-B","MSPAM-M32"]
["REIKU-B","MSPAM-M40"]
["REIKU-B","MSPAM-M50"]
["REIKU-B","MSPAM-M63"]
["REIKU-B","MSPAM-P09"]
["REIKU-B","MSPAM-P11"]
["REIKU-B","MSPAM-P16"]
["REIKU-B","MSPAM-P21"]
["REIKU-B","MSPAM-P29"]
["REIKU-B","MSPAM-P36"]
["REIKU-B","MSPAM-P42"]
["REIKU-B","MSPAM-P48"]
["TECHNIK","Multipěnový sprej"]
["TECHNIK SPECIAL - AKCIA","MW 10-C"]
["TECHNIK SPECIAL - AKCIA","MW 16-C"]
["TECHNIK SPECIAL - AKCIA","MW 25-C"]
["TECHNIK SPECIAL - AKCIA","MW 35-C"]
["TECHNIK SPECIAL - AKCIA","MW 50-C"]
["TECHNIK SPECIAL - AKCIA","MW 70-C"]
["TECHNIK SPECIAL - AKCIA","MW 95-C"]
["TECHNIK SPECIAL - AKCIA","MW120-C"]
["TECHNIK SPECIAL - AKCIA","MW150-C"]
["TECHNIK SPECIAL - AKCIA","MW185-C"]
["TECHNIK SPECIAL - AKCIA","MW240-C"]
["TECHNIK SPECIAL - AKCIA","NC 1319"]
["TECHNIK SPECIAL - AKCIA","NC 1924"]
["TECHNIK SPECIAL - AKCIA","NC 2432"]
["TECHNIK SPECIAL - AKCIA","NC 3241"]
["TECHNIK SPECIAL - AKCIA","NCPP-10"]
["TECHNIK SPECIAL - AKCIA","NCPP-20"]
["TECHNIK","ND 68-M2,5"]
["TECHNIK","ND 68-M3"]
["TECHNIK","ND 68-M4"]
["TECHNIK","ND 68-M4/5000"]
["TECHNIK","ND 68-M4-90"]
["TECHNIK","ND 68-M5"]
["TECHNIK","ND 68-M5-90"]
["TECHNIK","ND 68-M6"]
["TECHNIK","NDC 28-M3"]
["TECHNIK","NDC 68-M3"]
["TECHNIK","NDC 68-M3-90"]
["TECHNIK","NDC 68-M4"]
["TECHNIK","NDC 68-M4-90"]
["TECHNIK","NDC 68-M5"]
["TECHNIK","NDC 68-M6"]
["REIKU-B","NIDRB-17"]
["REIKU-B","NIDRB-23"]
["REIKU-B","NIDRB-29"]
["REIKU-B","NIDRB-36"]
["REIKU-B","NIDRB-48"]
["REIKU-B","NIFSB-52"]
["REIKU-B","NIFSB-70"]
["REIKU-B","NIFSB-95"]
["TECHNIK","NK 13"]
["TECHNIK","NK 13 H - MK9"]
["TECHNIK","NK 46"]
["TECHNIK","NK 48"]
["TECHNIK","NK 48 H - EVO7"]
["TECHNIK","NK 48 P - GS2B"]
["TECHNIK","NK 48 P - GTS"]
["TECHNIK","NK 9"]
["TECHNIK","NK 9 P - GTH"]
["TECHNIK","NKST 12"]
["TECHNIK","NKST 8"]
["TECHNIK","NL  10-M 4"]
["TECHNIK","NL  10-M 5"]
["TECHNIK","NL  10-M 6"]
["TECHNIK","NL  10-M 8"]
["TECHNIK","NL  10-M10"]
["TECHNIK","NL  10-M12"]
["TECHNIK","NL  16-M 4"]
["TECHNIK","NL  16-M 5"]
["TECHNIK","NL  16-M 6"]
["TECHNIK","NL  16-M 8"]
["TECHNIK","NL  16-M10"]
["TECHNIK","NL  16-M12"]
["TECHNIK","NL  25-M 5"]
["TECHNIK","NL  25-M 6"]
["TECHNIK","NL  25-M 8"]
["TECHNIK","NL  25-M10"]
["TECHNIK","NL  25-M12"]
["TECHNIK","NL  35-M 6"]
["TECHNIK","NL  35-M 8"]
["TECHNIK","NL  35-M10"]
["TECHNIK","NL  35-M12"]
["TECHNIK","NL  50-M 6"]
["TECHNIK","NL  50-M 8"]
["TECHNIK","NL  50-M10"]
["TECHNIK","NL  50-M12"]
["TECHNIK","NL  70-M 8"]
["TECHNIK","NL  70-M10"]
["TECHNIK","NL  70-M12"]
["TECHNIK","NL  95-M 8"]
["TECHNIK","NL  95-M10"]
["TECHNIK","NL  95-M12"]
["TECHNIK","NL 120-M10"]
["TECHNIK","NL 120-M12"]
["TECHNIK","NL 150-M12"]
["TECHNIK","NOALOX"]
["TECHNIK SPECIAL - AKCIA","NP 100 U"]
["TECHNIK SPECIAL - AKCIA","NP7-700"]
["TECHNIK SPECIAL - AKCIA","NP7-850"]
["TECHNIK","NR 68-M3"]
["TECHNIK","NR 68-M4"]
["TECHNIK","NR 68-M5"]
["TECHNIK","NRC 28-M2"]
["TECHNIK","NRC 48-M3"]
["TECHNIK","NRC 68-M3"]
["TECHNIK","NRC 68-M4"]
["TECHNIK","NRC 68-M5"]
["TECHNIK","NS 68-M3"]
["TECHNIK","NS 68-M4"]
["TECHNIK","NS 68-M5"]
["TECHNIK","NSC 68-M3"]
["TECHNIK","NSC 68-M4"]
["TECHNIK","NU 45-M3,5"]
["TECHNIK","NU 45-M4"]
["TECHNIK","NU 45-M5"]
["TECHNIK","NU 68-M3"]
["TECHNIK","NU 68-M4"]
["TECHNIK","NU 68-M4-90"]
["TECHNIK","NU 68-M5"]
["TECHNIK","NU 68-M6"]
["TECHNIK","NUC 28-M3-60"]
["TECHNIK","NUC 28-M3-90"]
["TECHNIK","NUC 45-M3,5"]
["TECHNIK","NUC 45-M4"]
["TECHNIK","NUC 45-M5"]
["TECHNIK","NUC 48-M3"]
["TECHNIK","NUC 48-M4"]
["TECHNIK","NUC 68-M3"]
["TECHNIK","NUC 68-M3-90"]
["TECHNIK","NUC 68-M4"]
["TECHNIK","NUC 68-M4-90"]
["TECHNIK","NUC 68-M5"]
["TECHNIK","NUC 68-M5-90"]
["TECHNIK","NUC 68-M5-90-O"]
["TECHNIK","NUC 68-M6"]
["TECHNIK","NUC 68-M8"]
["TECHNIK","NUN 2x68"]
["TECHNIK","NUN 2x68-M4"]
["TECHNIK","NUN 4x68-M3"]
["TECHNIK","NUN 68"]
["TECHNIK","Nůž ML 18"]
["TECHNIK","Nůž MP 9"]
["TECHNIK","Nůž PE  9"]
["TECHNIK","Nůž PE 18"]
["TECHNIK","Nůž PT  9"]
["TECHNIK","Nůž PT 18"]
["TECHNIK","Nůž PT 18 EXTREM"]
["TECHNIK","Nůž PT-V"]
["TECHNIK","Nůž ST  9"]
["TECHNIK","Nůž ST 18"]
["TECHNIK","Nůž ST-V"]
["TECHNIK","NYT 1x68-45"]
["TECHNIK","NYT 2x68-45"]
["TECHNIK","NYT 2x68-90"]
["TECHNIK","NYT 4x68-90"]
["TECHNIK","NYTC 1x68-90"]
["TECHNIK","Oddělovač forem"]
["TECHNIK","Odstraňovač etiket"]
["TECHNIK","Odstraňovač sprej"]
["TECHNIK","OF 22-M 8"]
["TECHNIK","OF 38-M 8"]
["TECHNIK","OF 70-M 8"]
["TECHNIK","Ochr. při svařování"]
["TECHNIK","Ochrana nerezu"]
["TECHNIK","OI  0,5-M 2,5/PA"]
["TECHNIK","OI  0,5-M 2/PA"]
["TECHNIK","OI  0,5-M 3,5/PA"]
["TECHNIK","OI  0,5-M 3/PA"]
["TECHNIK","OI  0,5-M 4/PA"]
["TECHNIK","OI  0,5-M 5/PA"]
["TECHNIK","OI  1,5-M 2,5"]
["TECHNIK","OI  1,5-M 2,5/E"]
["TECHNIK","OI  1,5-M 3"]
["TECHNIK","OI  1,5-M 3,5"]
["TECHNIK","OI  1,5-M 3,5/E"]
["TECHNIK","OI  1,5-M 3,5/PA"]
["TECHNIK","OI  1,5-M 3,5/PC"]
["TECHNIK","OI  1,5-M 3/E"]
["TECHNIK","OI  1,5-M 3/PA"]
["TECHNIK","OI  1,5-M 3/PC"]
["TECHNIK","OI  1,5-M 3/PK"]
["TECHNIK","OI  1,5-M 4"]
["TECHNIK","OI  1,5-M 4/7"]
["TECHNIK","OI  1,5-M 4/7/E"]
["TECHNIK","OI  1,5-M 4/E"]
["TECHNIK","OI  1,5-M 4/PA"]
["TECHNIK","OI  1,5-M 4/PC"]
["TECHNIK","OI  1,5-M 4/PK"]
["TECHNIK","OI  1,5-M 5"]
["TECHNIK","OI  1,5-M 5/10"]
["TECHNIK","OI  1,5-M 5/10/E"]
["TECHNIK","OI  1,5-M 5/10/PA"]
["TECHNIK","OI  1,5-M 5/10/PC"]
["TECHNIK","OI  1,5-M 5/10/PK"]
["TECHNIK","OI  1,5-M 5/E"]
["TECHNIK","OI  1,5-M 5/PA"]
["TECHNIK","OI  1,5-M 6"]
["TECHNIK","OI  1,5-M 6/E"]
["TECHNIK","OI  1,5-M 6/PA"]
["TECHNIK","OI  1,5-M 6/PK"]
["TECHNIK","OI  1,5-M 8"]
["TECHNIK","OI  1,5-M 8/14"]
["TECHNIK","OI  1,5-M 8/14/E"]
["TECHNIK","OI  1,5-M 8/14/PA"]
["TECHNIK","OI  1,5-M 8/PA"]
["TECHNIK","OI  1,5-M 8/PC"]
["TECHNIK","OI  1,5-M 8/PK"]
["TECHNIK","OI  1,5-M10"]
["TECHNIK","OI  1,5-M10/18"]
["TECHNIK","OI  1,5-M10/18/E"]
["TECHNIK","OI  1,5-M10/18/PA"]
["TECHNIK","OI  1,5-M10/18/PC"]
["TECHNIK","OI  1,5-M10/18/PK"]
["TECHNIK","OI  1,5-M10/E"]
["TECHNIK","OI  1,5-M12"]
["TECHNIK","OI  1,5-M12/E"]
["TECHNIK","OI  1,5-M16"]
["TECHNIK","OI  1,5-M20"]
["TECHNIK","OI  2,5-M 3"]
["TECHNIK","OI  2,5-M 3,5"]
["TECHNIK","OI  2,5-M 3,5/E"]
["TECHNIK","OI  2,5-M 3,5/PA"]
["TECHNIK","OI  2,5-M 3,5/PC"]
["TECHNIK","OI  2,5-M 3/E"]
["TECHNIK","OI  2,5-M 3/PA"]
["TECHNIK","OI  2,5-M 3/PC"]
["TECHNIK","OI  2,5-M 3/PK"]
["TECHNIK","OI  2,5-M 4"]
["TECHNIK","OI  2,5-M 4/7"]
["TECHNIK","OI  2,5-M 4/8,5"]
["TECHNIK","OI  2,5-M 4/E"]
["TECHNIK","OI  2,5-M 4/PA"]
["TECHNIK","OI  2,5-M 4/PC"]
["TECHNIK","OI  2,5-M 4/PK"]
["TECHNIK","OI  2,5-M 5"]
["TECHNIK","OI  2,5-M 5/8"]
["TECHNIK","OI  2,5-M 5/8/E"]
["TECHNIK","OI  2,5-M 5/E"]
["TECHNIK","OI  2,5-M 5/PA"]
["TECHNIK","OI  2,5-M 5/PA role"]
["TECHNIK","OI  2,5-M 5/PC"]
["TECHNIK","OI  2,5-M 5/PK"]
["TECHNIK","OI  2,5-M 6"]
["TECHNIK","OI  2,5-M 6/12/E"]
["TECHNIK","OI  2,5-M 6/E"]
["TECHNIK","OI  2,5-M 6/PA"]
["TECHNIK","OI  2,5-M 6/PC"]
["TECHNIK","OI  2,5-M 6/PK"]
["TECHNIK","OI  2,5-M 8"]
["TECHNIK","OI  2,5-M 8/14"]
["TECHNIK","OI  2,5-M 8/14/E"]
["TECHNIK","OI  2,5-M 8/14/PA"]
["TECHNIK","OI  2,5-M 8/14/PC"]
["TECHNIK","OI  2,5-M 8/14/PK"]
["TECHNIK","OI  2,5-M 8/E"]
["TECHNIK","OI  2,5-M 8/PA"]
["TECHNIK","OI  2,5-M10"]
["TECHNIK","OI  2,5-M10/18"]
["TECHNIK","OI  2,5-M10/18/E"]
["TECHNIK","OI  2,5-M10/18/PA"]
["TECHNIK","OI  2,5-M10/18/PC"]
["TECHNIK","OI  2,5-M10/18/PK"]
["TECHNIK","OI  2,5-M10/E"]
["TECHNIK","OI  2,5-M12"]
["TECHNIK","OI  2,5-M12/E"]
["TECHNIK","OI  2,5-M12/PA"]
["TECHNIK","OI  2,5-M12/PC"]
["TECHNIK","OI  2,5-M12/PK"]
["TECHNIK","OI  2,5-M16"]
["TECHNIK","OI  2,5-M20"]
["TECHNIK","OI  6-M 3"]
["TECHNIK","OI  6-M 3,5"]
["TECHNIK","OI  6-M 3,5/E"]
["TECHNIK","OI  6-M 3,5/PC"]
["TECHNIK","OI  6-M 3/E"]
["TECHNIK","OI  6-M 3/PA"]
["TECHNIK","OI  6-M 3/PC"]
["TECHNIK","OI  6-M 4"]
["TECHNIK","OI  6-M 4/7"]
["TECHNIK","OI  6-M 4/7/E"]
["TECHNIK","OI  6-M 4/8"]
["TECHNIK","OI  6-M 4/8/E"]
["TECHNIK","OI  6-M 4/E"]
["TECHNIK","OI  6-M 4/PA"]
["TECHNIK","OI  6-M 4/PC"]
["TECHNIK","OI  6-M 4/PK"]
["TECHNIK","OI  6-M 5"]
["TECHNIK","OI  6-M 5/E"]
["TECHNIK","OI  6-M 5/PA"]
["TECHNIK","OI  6-M 5/PC"]
["TECHNIK","OI  6-M 5/PK"]
["TECHNIK","OI  6-M 6"]
["TECHNIK","OI  6-M 6/E"]
["TECHNIK","OI  6-M 6/PA"]
["TECHNIK","OI  6-M 6/PC"]
["TECHNIK","OI  6-M 6/PK"]
["TECHNIK","OI  6-M 8"]
["TECHNIK","OI  6-M 8/E"]
["TECHNIK","OI  6-M 8/PA"]
["TECHNIK","OI  6-M 8/PK"]
["TECHNIK","OI  6-M10"]
["TECHNIK","OI  6-M10/18"]
["TECHNIK","OI  6-M10/18/E"]
["TECHNIK","OI  6-M10/18/PA"]
["TECHNIK","OI  6-M10/18/PC"]
["TECHNIK","OI  6-M10/18/PK"]
["TECHNIK","OI  6-M10/E"]
["TECHNIK","OI  6-M12"]
["TECHNIK","OI  6-M12/E"]
["TECHNIK","OI  6-M12/PA"]
["TECHNIK","OI  6-M12/PK"]
["TECHNIK","OI  6-M16"]
["TECHNIK","OI  6-M16/32"]
["TECHNIK","OI  6-M16/PA"]
["TECHNIK","OI  6-M20"]
["TECHNIK","OI 10-M 5/PA"]
["TECHNIK","OI 10-M 6/PA"]
["TECHNIK","OI 10-M 8/PA"]
["TECHNIK","OI 10-M10/PA"]
["TECHNIK","OI 10-M12/PA"]
["TECHNIK","OI 16-M 5/PA"]
["TECHNIK","OI 16-M 6/PA"]
["TECHNIK","OI 16-M 8/PA"]
["TECHNIK","OI 16-M10/PA"]
["TECHNIK","OI 16-M12/PA"]
["TECHNIK","OI 25-M 5/PA"]
["TECHNIK","OI 25-M 6/PA"]
["TECHNIK","OI 25-M 8/PA"]
["TECHNIK","OI 25-M10/PA"]
["TECHNIK","OI 25-M12/PA"]
["TECHNIK","OI 25-M16/PA"]
["TECHNIK","OI 35-M 8/PA"]
["TECHNIK","OI 35-M10/PA"]
["TECHNIK","OI 35-M12/PA"]
["TECHNIK","OI 50-M 8/PA"]
["TECHNIK","OI 50-M10/PA"]
["TECHNIK","OI 50-M12/PA"]
["TECHNIK","OI 95-M10/PA"]
["TECHNIK","OIS 1,5-M 2,5"]
["TECHNIK","OIS 1,5-M 3"]
["TECHNIK","OIS 1,5-M 3,5"]
["TECHNIK","OIS 1,5-M 4"]
["TECHNIK","OIS 1,5-M 4/7"]
["TECHNIK","OIS 1,5-M 5"]
["TECHNIK","OIS 1,5-M 5/8"]
["TECHNIK","OIS 1,5-M 6"]
["TECHNIK","OIS 1,5-M 8"]
["TECHNIK","OIS 1,5-M 8/12"]
["TECHNIK","OIS 1,5-M10"]
["TECHNIK","OIS 1,5-M10/15"]
["TECHNIK","OIS 2,5-M 3"]
["TECHNIK","OIS 2,5-M 3,5"]
["TECHNIK","OIS 2,5-M 4"]
["TECHNIK","OIS 2,5-M 4/7"]
["TECHNIK","OIS 2,5-M 5"]
["TECHNIK","OIS 2,5-M 5/8"]
["TECHNIK","OIS 2,5-M 6"]
["TECHNIK","OIS 2,5-M 8"]
["TECHNIK","OIS 2,5-M 8/12"]
["TECHNIK","OIS 2,5-M10"]
["TECHNIK","OIS 2,5-M10/15"]
["TECHNIK","OIS 2,5-M12"]
["TECHNIK","OIS 6-M 3"]
["TECHNIK","OIS 6-M 3,5"]
["TECHNIK","OIS 6-M 4"]
["TECHNIK","OIS 6-M 4/10"]
["TECHNIK","OIS 6-M 5"]
["TECHNIK","OIS 6-M 6"]
["TECHNIK","OIS 6-M 8"]
["TECHNIK","OIS 6-M10"]
["TECHNIK","OIS 6-M10/15"]
["TECHNIK","OIS 6-M12"]
["TECHNIK","OKC 1,5-4"]
["TECHNIK","OKC 1,5-4/PA"]
["TECHNIK","OKC 1,5-4/PC"]
["TECHNIK","OKC 2,5-4"]
["TECHNIK","OKC 2,5-4/PA"]
["TECHNIK","OKC 2,5-4/PC"]
["TECHNIK","OKC 2,5-5"]
["TECHNIK","OKC 2,5-5/PC"]
["TECHNIK","OKC 6-5"]
["TECHNIK","OKC 6-5/PC"]
["TECHNIK","OKP 1,5-4"]
["TECHNIK","OKP 1,5-4/PA"]
["TECHNIK","OKP 2,5-4"]
["TECHNIK","OKP 2,5-4/PA"]
["TECHNIK","OKP 2,5-5"]
["TECHNIK","OKP 2,5-5/PA"]
["TECHNIK","OKP 6-5"]
["TECHNIK","OKP 6-5/PA"]
["TECHNIK","OL  0,75-M 3"]
["TECHNIK","OL  0,75-M 4"]
["TECHNIK","OL  0,75-M 5"]
["TECHNIK","OL  1,5-M 3"]
["TECHNIK","OL  1,5-M 4"]
["TECHNIK","OL  1,5-M 5"]
["TECHNIK","OL  1,5-M 6"]
["TECHNIK","OL  2,5-M 3"]
["TECHNIK","OL  2,5-M 4"]
["TECHNIK","OL  2,5-M 5"]
["TECHNIK","OL  2,5-M 6"]
["TECHNIK","OL  2,5-M 8"]
["TECHNIK","OL  4-M 4"]
["TECHNIK","OL  4-M 5"]
["TECHNIK","OL  4-M 6"]
["TECHNIK","OL  4-M 8"]
["TECHNIK","OL  4-M10 "]
["TECHNIK","OL  6-M 4"]
["TECHNIK","OL  6-M 5"]
["TECHNIK","OL  6-M 6"]
["TECHNIK","OL  6-M 8"]
["TECHNIK","OL  6-M10"]
["TECHNIK","OL  6-M12"]
["TECHNIK","OL 10-M 4"]
["TECHNIK","OL 10-M 5"]
["TECHNIK","OL 10-M 6"]
["TECHNIK","OL 10-M 8"]
["TECHNIK","OL 10-M10"]
["TECHNIK","OL 10-M12"]
["TECHNIK","OL 16-M 4"]
["TECHNIK","OL 16-M 5"]
["TECHNIK","OL 16-M 5/F"]
["TECHNIK","OL 16-M 6"]
["TECHNIK","OL 16-M 6/S"]
["TECHNIK","OL 16-M 8"]
["TECHNIK","OL 16-M 8/F"]
["TECHNIK","OL 16-M 8/S"]
["TECHNIK","OL 16-M10"]
["TECHNIK","OL 16-M12"]
["TECHNIK","OL 16-M12/S"]
["TECHNIK","OL 16-M16"]
["TECHNIK","OL 25-M 5"]
["TECHNIK","OL 25-M 6"]
["TECHNIK","OL 25-M 6/S"]
["TECHNIK","OL 25-M 8"]
["TECHNIK","OL 25-M 8/F"]
["TECHNIK","OL 25-M10"]
["TECHNIK","OL 25-M10/F"]
["TECHNIK","OL 25-M10/S"]
["TECHNIK","OL 25-M12"]
["TECHNIK","OL 25-M12/F"]
["TECHNIK","OL 25-M16"]
["TECHNIK","OL 35"]
["TECHNIK","OL 35-M 6"]
["TECHNIK","OL 35-M 6/F"]
["TECHNIK","OL 35-M 6/S"]
["TECHNIK","OL 35-M 8"]
["TECHNIK","OL 35-M 8/F"]
["TECHNIK","OL 35-M 8/S"]
["TECHNIK","OL 35-M10"]
["TECHNIK","OL 35-M10/S"]
["TECHNIK","OL 35-M12"]
["TECHNIK","OL 35-M12/S"]
["TECHNIK","OL 35-M14"]
["TECHNIK","OL 35-M16"]
["TECHNIK","OL 35-M20"]
["TECHNIK","OL 50-M 6"]
["TECHNIK","OL 50-M 8"]
["TECHNIK","OL 50-M 8/S"]
["TECHNIK","OL 50-M10"]
["TECHNIK","OL 50-M12"]
["TECHNIK","OL 50-M12/F"]
["TECHNIK","OL 50-M12/S"]
["TECHNIK","OL 50-M16"]
["TECHNIK","OL 50-M20"]
["TECHNIK","OL 70"]
["TECHNIK","OL 70-M 6"]
["TECHNIK","OL 70-M 8"]
["TECHNIK","OL 70-M10"]
["TECHNIK","OL 70-M12"]
["TECHNIK","OL 70-M12/S"]
["TECHNIK","OL 70-M16"]
["TECHNIK","OL 70-M20"]
["TECHNIK","OL 95"]
["TECHNIK","OL 95-M 8"]
["TECHNIK","OL 95-M 8/F"]
["TECHNIK","OL 95-M10"]
["TECHNIK","OL 95-M10/S"]
["TECHNIK","OL 95-M12"]
["TECHNIK","OL 95-M12/S"]
["TECHNIK","OL 95-M14"]
["TECHNIK","OL 95-M16"]
["TECHNIK","OL 95-M16/S"]
["TECHNIK","OL 95-M20"]
["TECHNIK","OL120"]
["TECHNIK","OL120-M 6"]
["TECHNIK","OL120-M 8"]
["TECHNIK","OL120-M10"]
["TECHNIK","OL120-M12"]
["TECHNIK","OL120-M12/S"]
["TECHNIK","OL120-M16"]
["TECHNIK","OL120-M20"]
["TECHNIK","OL150"]
["TECHNIK","OL150-M 8"]
["TECHNIK","OL150-M10"]
["TECHNIK","OL150-M12"]
["TECHNIK","OL150-M16"]
["TECHNIK","OL150-M20"]
["TECHNIK","OL185-M 8"]
["TECHNIK","OL185-M10"]
["TECHNIK","OL185-M12"]
["TECHNIK","OL185-M16"]
["TECHNIK","OL185-M20"]
["TECHNIK","OL240-2xM12/25"]
["TECHNIK","OL240-M10"]
["TECHNIK","OL240-M12"]
["TECHNIK","OL240-M16"]
["TECHNIK","OL300-M12"]
["TECHNIK","OL300-M16"]
["TECHNIK","OL300-M20"]
["TECHNIK","OL400-M12"]
["TECHNIK","OL400-M16"]
["TECHNIK","OL400-M20"]
["TECHNIK","OL45R 10-M 8"]
["TECHNIK","OL45R 16-M 8"]
["TECHNIK","OL45R 25-M 8"]
["TECHNIK","OL45R 35-M 8"]
["TECHNIK","OL45R 35-M12"]
["TECHNIK","OL45R 35-M16"]
["TECHNIK","OL45R 50-M10"]
["TECHNIK","OL45R 70-M12"]
["TECHNIK","OL45R 95-M 8"]
["TECHNIK","OL45R240-M12"]
["TECHNIK","OL500-M12"]
["TECHNIK","OL500-M16"]
["TECHNIK","OL90R  6-M 4"]
["TECHNIK","OL90R  6-M 5"]
["TECHNIK","OL90R  6-M 6"]
["TECHNIK","OL90R  6-M 8"]
["TECHNIK","OL90R  6-M10"]
["TECHNIK","OL90R 10-M 5"]
["TECHNIK","OL90R 10-M 6"]
["TECHNIK","OL90R 10-M 8"]
["TECHNIK","OL90R 10-M10"]
["TECHNIK","OL90R 16-M 5"]
["TECHNIK","OL90R 16-M 6"]
["TECHNIK","OL90R 16-M 8"]
["TECHNIK","OL90R 16-M10"]
["TECHNIK","OL90R 16-M12"]
["TECHNIK","OL90R 25-M 6"]
["TECHNIK","OL90R 25-M 8"]
["TECHNIK","OL90R 25-M10"]
["TECHNIK","OL90R 25-M12"]
["TECHNIK","OL90R 35-M 6"]
["TECHNIK","OL90R 35-M 8"]
["TECHNIK","OL90R 35-M10"]
["TECHNIK","OL90R 35-M12"]
["TECHNIK","OL90R 35-M16"]
["TECHNIK","OL90R 50-M 6"]
["TECHNIK","OL90R 50-M 8"]
["TECHNIK","OL90R 50-M10"]
["TECHNIK","OL90R 50-M12"]
["TECHNIK","OL90R 50-M16"]
["TECHNIK","OL90R 70-M 8"]
["TECHNIK","OL90R 70-M10"]
["TECHNIK","OL90R 70-M12"]
["TECHNIK","OL90R 70-M16"]
["TECHNIK","OL90R 95-M 8"]
["TECHNIK","OL90R 95-M10"]
["TECHNIK","OL90R 95-M12"]
["TECHNIK","OL90R 95-M16"]
["TECHNIK","OL90R120-M 8"]
["TECHNIK","OL90R120-M10"]
["TECHNIK","OL90R120-M12"]
["TECHNIK","OL90R120-M16"]
["TECHNIK","OL90R150-M 8"]
["TECHNIK","OL90R150-M12"]
["TECHNIK","OL90R185-M12"]
["TECHNIK","OL90R240-M12"]
["TECHNIK","OL90R240-M16"]
["TECHNIK SPECIAL - AKCIA","OLEJ HF-E15"]
["TECHNIK SPECIAL - AKCIA","OLEJ H-LP46"]
["TECHNIK","OLN  1,5-M4"]
["TECHNIK","OLN  1,5-M5"]
["TECHNIK","OLN  2,5-M4"]
["TECHNIK","OLN  2,5-M5"]
["TECHNIK","OLN  2,5-M6"]
["TECHNIK","OLN  6-M4"]
["TECHNIK","OLN  6-M5"]
["TECHNIK","OLN  6-M6"]
["TECHNIK","OLN 25-M8"]
["TECHNIK","OLN 50-M8"]
["TECHNIK","OLN 70-M10"]
["TECHNIK","OLN 95-M10"]
["TECHNIK","OLN 95-M12"]
["TECHNIK","OLNO  2,5-M4"]
["TECHNIK","OLNO  2,5-M5"]
["TECHNIK","OLNO  2,5-M6"]
["TECHNIK","OLNO  6-M4"]
["TECHNIK","OLNO  6-M5"]
["TECHNIK","OLNO  6-M6"]
["TECHNIK","OLNO 10-M6"]
["TECHNIK","OLNO 10-M8"]
["TECHNIK","OLNO 16-M5"]
["TECHNIK","OLNO 16-M6"]
["TECHNIK","OLNO 16-M8"]
["TECHNIK","OLNO 50-M8"]
["TECHNIK","ON  0,5-M 2"]
["TECHNIK","ON  0,5-M 2,5"]
["TECHNIK","ON  0,5-M 3"]
["TECHNIK","ON  0,5-M 3,5"]
["TECHNIK","ON  0,5-M 4"]
["TECHNIK","ON  0,5-M 5"]
["TECHNIK","ON  1,5-M 2"]
["TECHNIK","ON  1,5-M 2,5"]
["TECHNIK","ON  1,5-M 3"]
["TECHNIK","ON  1,5-M 3,5"]
["TECHNIK","ON  1,5-M 4"]
["TECHNIK","ON  1,5-M 5"]
["TECHNIK","ON  1,5-M 5/8"]
["TECHNIK","ON  1,5-M 6"]
["TECHNIK","ON  1,5-M 8"]
["TECHNIK","ON  1,5-M10"]
["TECHNIK","ON  1,5-M12"]
["TECHNIK","ON  1,5-M16"]
["TECHNIK","ON  1,5-M20"]
["TECHNIK","ON  2,5-M 3"]
["TECHNIK","ON  2,5-M 3,5"]
["TECHNIK","ON  2,5-M 4"]
["TECHNIK","ON  2,5-M 5"]
["TECHNIK","ON  2,5-M 6"]
["TECHNIK","ON  2,5-M 8"]
["TECHNIK","ON  2,5-M 8/12"]
["TECHNIK","ON  2,5-M10"]
["TECHNIK","ON  2,5-M10/15"]
["TECHNIK","ON  2,5-M12"]
["TECHNIK","ON  2,5-M16"]
["TECHNIK","ON  2,5-M20"]
["TECHNIK","ON  6-M 3"]
["TECHNIK","ON  6-M 3,5"]
["TECHNIK","ON  6-M 4"]
["TECHNIK","ON  6-M 5"]
["TECHNIK","ON  6-M 6"]
["TECHNIK","ON  6-M 8"]
["TECHNIK","ON  6-M10"]
["TECHNIK","ON  6-M12"]
["TECHNIK","ON  6-M16"]
["TECHNIK","ON  6-M16/32"]
["TECHNIK","ON  6-M20"]
["TECHNIK","ON 10-M 4"]
["TECHNIK","ON 10-M 5"]
["TECHNIK","ON 10-M 6"]
["TECHNIK","ON 10-M 8"]
["TECHNIK","ON 10-M10"]
["TECHNIK","ON 10-M12"]
["TECHNIK","ON 10-M16"]
["TECHNIK","ON 10-M20"]
["TECHNIK","ON 16-M 5"]
["TECHNIK","ON 16-M 6"]
["TECHNIK","ON 16-M 8"]
["TECHNIK","ON 16-M10"]
["TECHNIK","ON 16-M12"]
["TECHNIK","ON 16-M16"]
["TECHNIK","ON 16-M20"]
["TECHNIK","ON 25-M 5"]
["TECHNIK","ON 25-M 6"]
["TECHNIK","ON 25-M 8"]
["TECHNIK","ON 25-M10"]
["TECHNIK","ON 25-M12"]
["TECHNIK","ON 25-M16"]
["TECHNIK","ON 25-M20"]
["TECHNIK","ON 35-M 6"]
["TECHNIK","ON 35-M 8"]
["TECHNIK","ON 35-M10"]
["TECHNIK","ON 35-M12"]
["TECHNIK","ON 35-M16"]
["TECHNIK","ON 35-M20"]
["TECHNIK","ON 50-M 6"]
["TECHNIK","ON 50-M 8"]
["TECHNIK","ON 50-M10"]
["TECHNIK","ON 50-M12"]
["TECHNIK","ON 50-M16"]
["TECHNIK","ON 50-M20"]
["TECHNIK","ON 70-M 6"]
["TECHNIK","ON 70-M 8"]
["TECHNIK","ON 70-M10"]
["TECHNIK","ON 70-M12"]
["TECHNIK","ON 70-M16"]
["TECHNIK","ON 70-M20"]
["TECHNIK","ON 95-M 8"]
["TECHNIK","ON 95-M10"]
["TECHNIK","ON 95-M12"]
["TECHNIK","ON 95-M16"]
["TECHNIK","ON120-M 8"]
["TECHNIK","ON120-M10"]
["TECHNIK","ON120-M12"]
["TECHNIK","ON120-M16"]
["TECHNIK","ON120-M20"]
["TECHNIK","ON150-M10"]
["TECHNIK","ON150-M12"]
["TECHNIK","ON150-M16"]
["TECHNIK","ON185-M10"]
["TECHNIK","ON185-M12"]
["TECHNIK","ON185-M16"]
["TECHNIK","ON240-M10"]
["TECHNIK","ON240-M12"]
["TECHNIK","ON240-M16"]
["TECHNIK","ON300-M12"]
["TECHNIK","ONM 1,5-M 3"]
["TECHNIK","ONM 1,5-M 4"]
["TECHNIK","ONM 1,5-M 4/9"]
["TECHNIK","ONM 1,5-M 5"]
["TECHNIK","ONM 1,5-M 5/9"]
["TECHNIK","ONM 1,5-M 6"]
["TECHNIK","ONM 1,5-M 6/12"]
["TECHNIK","ONM 1,5-M 8"]
["TECHNIK","ONM 1,5-M10"]
["TECHNIK","ONM 2,5-M 4"]
["TECHNIK","ONM 2,5-M 5"]
["TECHNIK","ONM 2,5-M 6"]
["TECHNIK","ONM 2,5-M 6/12"]
["TECHNIK","ONM 2,5-M 8"]
["TECHNIK","ONM 2,5-M10"]
["TECHNIK","ONM 4-M 6"]
["TECHNIK","ONM 4-M 7"]
["TECHNIK","ONM 4-M 8"]
["TECHNIK","ONM 4-M 8/14"]
["TECHNIK","ONM 4-M10"]
["TECHNIK","ONM 6-M 4"]
["TECHNIK","ONMC 1,5-M 3"]
["TECHNIK","ONMC 1,5-M 3/9"]
["TECHNIK","ONMC 1,5-M 4"]
["TECHNIK","ONMC 1,5-M 4/9"]
["TECHNIK","ONMC 1,5-M 5"]
["TECHNIK","ONMC 1,5-M 5/9"]
["TECHNIK","ONMC 1,5-M 6"]
["TECHNIK","ONMC 1,5-M 6/12"]
["TECHNIK","ONMC 1,5-M 8"]
["TECHNIK","ONMC 2,5-M 3"]
["TECHNIK","ONMC 2,5-M 4"]
["TECHNIK","ONMC 2,5-M 5"]
["TECHNIK","ONMC 2,5-M 5/9"]
["TECHNIK","ONMC 2,5-M 6"]
["TECHNIK","ONMC 2,5-M 6/12"]
["TECHNIK","ONMC 2,5-M 8"]
["TECHNIK","ONMC 2,5-M 8/1"]
["TECHNIK","ONMC 2,5-M10"]
["TECHNIK","ONMC 2,5-M12"]
["TECHNIK","ONMC 4-M 6"]
["TECHNIK","ONMC 4-M 7"]
["TECHNIK","ONMC 4-M 8"]
["TECHNIK","ONMC 4-M 8/14"]
["TECHNIK","ONMC 4-M10"]
["TECHNIK","ONMC 6-M 4"]
["TECHNIK","ONMC 6-M 5"]
["TECHNIK","ONMC 6-M 6"]
["TECHNIK","ONMC 6-M 8"]
["TECHNIK","ONMC10-M 5"]
["TECHNIK","ONMC10-M 6"]
["TECHNIK","ONMC10-M 8"]
["TECHNIK","ONMC10-M10"]
["TECHNIK","OON 1,0-68"]
["TECHNIK","OON 2,5-68"]
["TECHNIK","OON 6-68"]
["TECHNIK","OP  6-10/2xM 6"]
["TECHNIK","OP  6-10/2xM 8"]
["TECHNIK","OP  6-10/2xM10"]
["TECHNIK SPECIAL - AKCIA","OP 100 D"]
["TECHNIK","OP 10-16/2xM 6"]
["TECHNIK","OP 10-16/2xM 8"]
["TECHNIK","OP 16-25/2xM 8"]
["TECHNIK","OP 16-25/2xM10"]
["TECHNIK","OP 16-25/4xM 6"]
["TECHNIK","OP 16-25/4xM 8"]
["TECHNIK","OP 16-25/4xM10"]
["TECHNIK","OP 16-25/4xM12"]
["TECHNIK SPECIAL - AKCIA","OP 200"]
["TECHNIK","OP 25-35/2xM 8"]
["TECHNIK","OP 25-35/4xM 8"]
["TECHNIK","OP 25-35/4xM10"]
["TECHNIK","OP 25-35/4xM12"]
["TECHNIK","OP 35-50/4xM 8"]
["TECHNIK","OP 35-50/4xM10"]
["TECHNIK","OP 35-50/4xM12"]
["TECHNIK","OP 50-70/4xM 8"]
["TECHNIK","OP 50-70/4xM10"]
["TECHNIK","OP 50-70/4xM12"]
["TECHNIK","OP 70- 95/4xM10"]
["TECHNIK","OP 70- 95/4xM12"]
["TECHNIK","OP 70-120/4xM10"]
["TECHNIK","OP 70-120/4xM12"]
["TECHNIK","OP 70-120/4xM16"]
["TECHNIK","OP 95-150/4xM10"]
["TECHNIK","OP 95-150/4xM12"]
["TECHNIK","OP 95-150/4xM16"]
["TECHNIK","OP150-240/4xM10"]
["TECHNIK","OP150-240/4xM12"]
["TECHNIK","OP150-240/4xM16"]
["TECHNIK","OP150-240/4xM20"]
["TECHNIK","OP185-300/4xM12"]
["TECHNIK","OPC 0,5-25/PA"]
["TECHNIK","OPC 0,5-28/PA"]
["TECHNIK","OPC 0,5-45/PA"]
["TECHNIK","OPC 0,5-48/PA"]
["TECHNIK","OPC 1,5-25"]
["TECHNIK","OPC 1,5-25/PA"]
["TECHNIK","OPC 1,5-25/PC"]
["TECHNIK","OPC 1,5-28"]
["TECHNIK","OPC 1,5-28/PA"]
["TECHNIK","OPC 1,5-28/PC"]
["TECHNIK","OPC 1,5-45"]
["TECHNIK","OPC 1,5-45/PC"]
["TECHNIK","OPC 1,5-48"]
["TECHNIK","OPC 1,5-48/PC"]
["TECHNIK","OPC 1,5-68"]
["TECHNIK","OPC 1,5-68 BP/PA"]
["TECHNIK","OPC 1,5-68 BP/PC"]
["TECHNIK","OPC 1,5-68/OBD"]
["TECHNIK","OPC 1,5-68/PA"]
["TECHNIK","OPC 1,5-68/PC"]
["TECHNIK","OPC 2,5-25/PA"]
["TECHNIK","OPC 2,5-28/PA"]
["TECHNIK","OPC 2,5-45"]
["TECHNIK","OPC 2,5-45/PC"]
["TECHNIK","OPC 2,5-48"]
["TECHNIK","OPC 2,5-48/PC"]
["TECHNIK","OPC 2,5-68"]
["TECHNIK","OPC 2,5-68 BP/PA"]
["TECHNIK","OPC 2,5-68 BP/PC"]
["TECHNIK","OPC 2,5-68/OBD"]
["TECHNIK","OPC 2,5-68/PA"]
["TECHNIK","OPC 2,5-68/PC"]
["TECHNIK","OPC 6-68"]
["TECHNIK","OPC 6-68 BP/PA"]
["TECHNIK","OPC 6-68/PA"]
["TECHNIK","OPC 6-68/PC"]
["TECHNIK","OPC 6-91"]
["TECHNIK","OPC 6-91/PC"]
["TECHNIK","OPCS 1,5-68"]
["TECHNIK","OPCS 2,5-68"]
["TECHNIK","OPCS 6-68"]
["TECHNIK","OPO 1,5"]
["TECHNIK","OPO 1,5/PA"]
["TECHNIK","OPO 1,5/PC"]
["TECHNIK","OPO 2,5"]
["TECHNIK","OPO 2,5/PA"]
["TECHNIK","OPO 2,5/PC"]
["TECHNIK","OPO 6"]
["TECHNIK","OPO 6/PC"]
["TECHNIK","OPOC 1,5"]
["TECHNIK","OPOC 2,5"]
["TECHNIK","OPP 0,5-25"]
["TECHNIK","OPP 0,5-28"]
["TECHNIK","OPP 1,5-25"]
["TECHNIK","OPP 1,5-25/PC"]
["TECHNIK","OPP 1,5-28"]
["TECHNIK","OPP 1,5-28/PC"]
["TECHNIK","OPP 1,5-45"]
["TECHNIK","OPP 1,5-45/PC"]
["TECHNIK","OPP 1,5-48"]
["TECHNIK","OPP 1,5-48 role"]
["TECHNIK","OPP 1,5-48/PA"]
["TECHNIK","OPP 1,5-48/PA role"]
["TECHNIK","OPP 1,5-48/PC"]
["TECHNIK","OPP 1,5-68"]
["TECHNIK","OPP 1,5-68/PA"]
["TECHNIK","OPP 1,5-68/PC"]
["TECHNIK","OPP 2,5-25"]
["TECHNIK","OPP 2,5-25/PA"]
["TECHNIK","OPP 2,5-25/PC"]
["TECHNIK","OPP 2,5-28"]
["TECHNIK","OPP 2,5-28/PC"]
["TECHNIK","OPP 2,5-45"]
["TECHNIK","OPP 2,5-45/PC"]
["TECHNIK","OPP 2,5-48"]
["TECHNIK","OPP 2,5-48/PA"]
["TECHNIK","OPP 2,5-48/PC"]
["TECHNIK","OPP 2,5-68"]
["TECHNIK","OPP 2,5-68/PA"]
["TECHNIK","OPP 2,5-68/PC"]
["TECHNIK","OPP 2,5-91"]
["TECHNIK","OPP 6-25"]
["TECHNIK","OPP 6-28"]
["TECHNIK","OPP 6-45"]
["TECHNIK","OPP 6-45/PC"]
["TECHNIK","OPP 6-48"]
["TECHNIK","OPP 6-48/PA"]
["TECHNIK","OPP 6-48/PC"]
["TECHNIK","OPP 6-68"]
["TECHNIK","OPP 6-68/PA"]
["TECHNIK","OPP 6-68/PC"]
["TECHNIK","OPP 6-91"]
["TECHNIK","OPP 6-91/PC"]
["TECHNIK","OPPS 1,5-25"]
["TECHNIK","OPPS 1,5-28"]
["TECHNIK","OPPS 1,5-45"]
["TECHNIK","OPPS 1,5-48"]
["TECHNIK","OPPS 1,5-68"]
["TECHNIK","OPPS 2,5-25"]
["TECHNIK","OPPS 2,5-28"]
["TECHNIK","OPPS 2,5-45"]
["TECHNIK","OPPS 2,5-48"]
["TECHNIK","OPPS 2,5-68"]
["TECHNIK","OPPS 6-45"]
["TECHNIK","OPPS 6-48"]
["TECHNIK","OPPS 6-68"]
["TECHNIK","Organizér M"]
["TECHNIK","Organizér V"]
["TECHNIK","OTR  7"]
["TECHNIK","OTR 11"]
["TECHNIK","OTR 13"]
["TECHNIK","OTR 15"]
["TECHNIK","OTR 19"]
["TECHNIK","OTR 22"]
["TECHNIK","OTR 25"]
["TECHNIK","OTR 28"]
["TECHNIK","OTR 32"]
["TECHNIK SPECIAL - AKCIA","P 19,0x 19,0"]
["TECHNIK SPECIAL - AKCIA","P 22,0x 42,0"]
["TECHNIK SPECIAL - AKCIA","P 22,2x 22,2"]
["TECHNIK SPECIAL - AKCIA","P 22,5/20,1"]
["TECHNIK SPECIAL - AKCIA","P 22,5/3"]
["TECHNIK SPECIAL - AKCIA","P 25,4x 25,4"]
["TECHNIK SPECIAL - AKCIA","P 36,0x 52,0"]
["TECHNIK SPECIAL - AKCIA","P 36,0x 65,0"]
["TECHNIK SPECIAL - AKCIA","P 36,0x 86,0"]
["TECHNIK SPECIAL - AKCIA","P 45,0x 45,0"]
["TECHNIK SPECIAL - AKCIA","P 45,0x 92,0"]
["TECHNIK SPECIAL - AKCIA","P 45,5x 45,5"]
["TECHNIK SPECIAL - AKCIA","P 46,0x 46,0"]
["TECHNIK SPECIAL - AKCIA","P 46,0x 92,0"]
["TECHNIK SPECIAL - AKCIA","P 60 CK"]
["TECHNIK SPECIAL - AKCIA","P 68,0x 68,0"]
["TECHNIK SPECIAL - AKCIA","P 68,0x 68,0 PLUS"]
["TECHNIK SPECIAL - AKCIA","P 68,0x138,0"]
["TECHNIK SPECIAL - AKCIA","P 92,0x 92,0"]
["TECHNIK","P A  1,0 P"]
["TECHNIK","P A  1,5"]
["TECHNIK","P A  1,5 P"]
["TECHNIK","P A  1,5 SET"]
["TECHNIK","P A  2,5"]
["TECHNIK","P A  2,5 P"]
["TECHNIK","P A  2,5 SET"]
["TECHNIK","P A  4"]
["TECHNIK","P A  4 P"]
["TECHNIK","P A  4 SET"]
["TECHNIK","P A  6"]
["TECHNIK","P A  6 P"]
["TECHNIK","P A  6 SET"]
["TECHNIK","P A 10"]
["TECHNIK","P A 10 P"]
["TECHNIK","P A 10 SET"]
["TECHNIK","P A 16"]
["TECHNIK","P A 16 P"]
["TECHNIK","P A 25 P"]
["TECHNIK","P A 25 SET"]
["TECHNIK","P A 70 P"]
["TECHNIK SPECIAL - AKCIA","P125,0x125,0"]
["REIKU-B","P2 connector NW07 with seal"]
["REIKU-B","P2 connector NW07 without seal"]
["REIKU-B","P2 connector NW10 with seal"]
["REIKU-B","P2 connector NW10 without seal"]
["REIKU-B","P2 connector NW12 with seal"]
["REIKU-B","P2 connector NW12 without seal"]
["REIKU-B","P2 connector NW17 with seal"]
["REIKU-B","P2 connector NW17 without seal"]
["REIKU-B","P2 connector NW23 with seal"]
["REIKU-B","P2 connector NW23 without seal"]
["REIKU-B","P2 connector NW29 with seal"]
["REIKU-B","P2 connector NW29 without seal"]
["TECHNIK","PA 02/12"]
["TECHNIK","PA 02/15"]
["TECHNIK","PA 02/21"]
["TECHNIK","PA 02/3"]
["TECHNIK","PA 02/3 euro 0-9"]
["TECHNIK","PA 02/3 žlutá 0-9"]
["TECHNIK","PA 02/3.09 \"+\""]
["TECHNIK","PA 02/3.09 \"0\"euro"]
["TECHNIK","PA 02/3.09 \"1\""]
["TECHNIK","PA 02/3.09 \"2\""]
["TECHNIK","PA 02/3.09 \"3\""]
["TECHNIK","PA 02/3.09 \"4\""]
["TECHNIK","PA 02/3.09 \"5\""]
["TECHNIK","PA 02/3.09 \"G\""]
["TECHNIK","PA 02/3.09 \"L\""]
["TECHNIK","PA 02/3.19 \"1\"euro"]
["TECHNIK","PA 02/3.29 \"+\""]
["TECHNIK","PA 02/3.29 \"2\"euro"]
["TECHNIK","PA 02/3.30 \"3\"euro"]
["TECHNIK","PA 02/3.4. 500"]
["TECHNIK","PA 02/3.40 \"-\""]
["TECHNIK","PA 02/3.40 \"-\" 1000"]
["TECHNIK","PA 02/3.40 \"-\" 500"]
["TECHNIK","PA 02/3.40 \".\""]
["TECHNIK","PA 02/3.40 \"/\""]
["TECHNIK","PA 02/3.40 \":\""]
["TECHNIK","PA 02/3.40 \"+\""]
["TECHNIK","PA 02/3.40 \"+\" 1000"]
["TECHNIK","PA 02/3.40 \"+\" 500"]
["TECHNIK","PA 02/3.40 \"0\""]
["TECHNIK","PA 02/3.40 \"0\" 1000"]
["TECHNIK","PA 02/3.40 \"0\" 500"]
["TECHNIK","PA 02/3.40 \"1\""]
["TECHNIK","PA 02/3.40 \"1\" 1000"]
["TECHNIK","PA 02/3.40 \"1\" 500"]
["TECHNIK","PA 02/3.40 \"2\""]
["TECHNIK","PA 02/3.40 \"2\" 1000"]
["TECHNIK","PA 02/3.40 \"2\" 500"]
["TECHNIK","PA 02/3.40 \"3\""]
["TECHNIK","PA 02/3.40 \"3\" 1000"]
["TECHNIK","PA 02/3.40 \"3\" 500"]
["TECHNIK","PA 02/3.40 \"4\" 1000"]
["TECHNIK","PA 02/3.40 \"4\" 500"]
["TECHNIK","PA 02/3.40 \"4\"euro"]
["TECHNIK","PA 02/3.40 \"5\""]
["TECHNIK","PA 02/3.40 \"5\" 1000"]
["TECHNIK","PA 02/3.40 \"5\" 500"]
["TECHNIK","PA 02/3.40 \"6\""]
["TECHNIK","PA 02/3.40 \"6\" 1000"]
["TECHNIK","PA 02/3.40 \"6\" 500"]
["TECHNIK","PA 02/3.40 \"7\""]
["TECHNIK","PA 02/3.40 \"7\" 1000"]
["TECHNIK","PA 02/3.40 \"7\" 500"]
["TECHNIK","PA 02/3.40 \"8\""]
["TECHNIK","PA 02/3.40 \"8\" 1000"]
["TECHNIK","PA 02/3.40 \"8\" 250"]
["TECHNIK","PA 02/3.40 \"8\" 500"]
["TECHNIK","PA 02/3.40 \"9\""]
["TECHNIK","PA 02/3.40 \"9\" 1000"]
["TECHNIK","PA 02/3.40 \"9\" 250"]
["TECHNIK","PA 02/3.40 \"9\" 500"]
["TECHNIK","PA 02/3.40 \"A\""]
["TECHNIK","PA 02/3.40 \"A\" 1000"]
["TECHNIK","PA 02/3.40 \"B\""]
["TECHNIK","PA 02/3.40 \"C\""]
["TECHNIK","PA 02/3.40 \"D\""]
["TECHNIK","PA 02/3.40 \"E\""]
["TECHNIK","PA 02/3.40 \"F\""]
["TECHNIK","PA 02/3.40 \"G\""]
["TECHNIK","PA 02/3.40 \"H\""]
["TECHNIK","PA 02/3.40 \"I\""]
["TECHNIK","PA 02/3.40 \"J\""]
["TECHNIK","PA 02/3.40 \"K\""]
["TECHNIK","PA 02/3.40 \"L\""]
["TECHNIK","PA 02/3.40 \"M\""]
["TECHNIK","PA 02/3.40 \"N\""]
["TECHNIK","PA 02/3.40 \"O\""]
["TECHNIK","PA 02/3.40 \"P\""]
["TECHNIK","PA 02/3.40 \"Q\""]
["TECHNIK","PA 02/3.40 \"R\""]
["TECHNIK","PA 02/3.40 \"S\""]
["TECHNIK","PA 02/3.40 \"T\""]
["TECHNIK","PA 02/3.40 \"T\" 1000"]
["TECHNIK","PA 02/3.40 \"U\""]
["TECHNIK","PA 02/3.40 \"U\" 1000"]
["TECHNIK","PA 02/3.40 \"V\""]
["TECHNIK","PA 02/3.40 \"V\" 1000"]
["TECHNIK","PA 02/3.40 \"W\""]
["TECHNIK","PA 02/3.40 \"W\" 1000"]
["TECHNIK","PA 02/3.40 \"X\""]
["TECHNIK","PA 02/3.40 \"Y\""]
["TECHNIK","PA 02/3.40 \"Z\""]
["TECHNIK","PA 02/3.40 \"zem\""]
["TECHNIK","PA 02/3.59 \"5\"euro"]
["TECHNIK","PA 02/3.69 \"-\""]
["TECHNIK","PA 02/3.69 \"6\"euro"]
["TECHNIK","PA 02/3.69 \"N\""]
["TECHNIK","PA 02/3.79 \"7\"euro"]
["TECHNIK","PA 02/3.8"]
["TECHNIK","PA 02/3.80 \"8\"euro"]
["TECHNIK","PA 02/3.90 \"1\""]
["TECHNIK","PA 02/3.90 \"2\""]
["TECHNIK","PA 02/3.90 \"3\""]
["TECHNIK","PA 02/3.90 \"4\""]
["TECHNIK","PA 02/3.90 \"5\""]
["TECHNIK","PA 02/3.90 \"6\""]
["TECHNIK","PA 02/3.90 \"7\""]
["TECHNIK","PA 02/3.90 \"8\""]
["TECHNIK","PA 02/3.90 \"9\"euro"]
["TECHNIK","PA 02/6"]
["TECHNIK","PA 02/6.40 \"L1\""]
["TECHNIK","PA 02/6.40 \"L2\""]
["TECHNIK","PA 02/6.40 \"L3\""]
["TECHNIK","PA 02/6.40 \"MP\""]
["TECHNIK","PA 02/6.40 \"PE\""]
["TECHNIK","PA 02/6.40 \"U1\""]
["TECHNIK","PA 02/6.40 \"U2\""]
["TECHNIK","PA 02/6.40 \"V1\""]
["TECHNIK","PA 02/6.40 \"V2\""]
["TECHNIK","PA 02/6.40 \"W1\""]
["TECHNIK","PA 02/6.40 \"W2\""]
["TECHNIK","PA 02/9"]
["TECHNIK","PA 1/12"]
["TECHNIK","PA 1/18"]
["TECHNIK","PA 1/21"]
["TECHNIK","PA 1/3"]
["TECHNIK","PA 1/3 euro 0-9"]
["TECHNIK","PA 1/3 žlutá 0-9"]
["TECHNIK","PA 1/3.09 \"0\"euro"]
["TECHNIK","PA 1/3.1 hnědá"]
["TECHNIK","PA 1/3.19 \"1\"euro"]
["TECHNIK","PA 1/3.29 \"+\""]
["TECHNIK","PA 1/3.29 \"+\" 1000"]
["TECHNIK","PA 1/3.29 \"0\""]
["TECHNIK","PA 1/3.29 \"1\""]
["TECHNIK","PA 1/3.29 \"2\"euro"]
["TECHNIK","PA 1/3.29 \"3\""]
["TECHNIK","PA 1/3.29 \"4\""]
["TECHNIK","PA 1/3.29 \"5\""]
["TECHNIK","PA 1/3.29 \"6\""]
["TECHNIK","PA 1/3.29 \"7\""]
["TECHNIK","PA 1/3.29 \"8\""]
["TECHNIK","PA 1/3.29 \"9\""]
["TECHNIK","PA 1/3.30 \"3\"euro"]
["TECHNIK","PA 1/3.4. 500"]
["TECHNIK","PA 1/3.40 \"-\""]
["TECHNIK","PA 1/3.40 \"-\" 500"]
["TECHNIK","PA 1/3.40 \".\""]
["TECHNIK","PA 1/3.40 \"/\""]
["TECHNIK","PA 1/3.40 \"+\""]
["TECHNIK","PA 1/3.40 \"+\" 500"]
["TECHNIK","PA 1/3.40 \"0\""]
["TECHNIK","PA 1/3.40 \"0\" 1000"]
["TECHNIK","PA 1/3.40 \"0\" 500"]
["TECHNIK","PA 1/3.40 \"1\""]
["TECHNIK","PA 1/3.40 \"1\" 1000"]
["TECHNIK","PA 1/3.40 \"1\" 500"]
["TECHNIK","PA 1/3.40 \"2\""]
["TECHNIK","PA 1/3.40 \"2\" 1000"]
["TECHNIK","PA 1/3.40 \"2\" 500"]
["TECHNIK","PA 1/3.40 \"3\""]
["TECHNIK","PA 1/3.40 \"3\" 1000"]
["TECHNIK","PA 1/3.40 \"3\" 500"]
["TECHNIK","PA 1/3.40 \"4\" 1000"]
["TECHNIK","PA 1/3.40 \"4\" 500"]
["TECHNIK","PA 1/3.40 \"4\"euro"]
["TECHNIK","PA 1/3.40 \"5\""]
["TECHNIK","PA 1/3.40 \"5\" 1000"]
["TECHNIK","PA 1/3.40 \"5\" 500"]
["TECHNIK","PA 1/3.40 \"6\""]
["TECHNIK","PA 1/3.40 \"6\" 1000"]
["TECHNIK","PA 1/3.40 \"6\" 500"]
["TECHNIK","PA 1/3.40 \"7\""]
["TECHNIK","PA 1/3.40 \"7\" 1000"]
["TECHNIK","PA 1/3.40 \"7\" 500"]
["TECHNIK","PA 1/3.40 \"8\""]
["TECHNIK","PA 1/3.40 \"8\" 1000"]
["TECHNIK","PA 1/3.40 \"8\" 500"]
["TECHNIK","PA 1/3.40 \"9\""]
["TECHNIK","PA 1/3.40 \"9\" 1000"]
["TECHNIK","PA 1/3.40 \"9\" 500"]
["TECHNIK","PA 1/3.40 \"A\""]
["TECHNIK","PA 1/3.40 \"B\""]
["TECHNIK","PA 1/3.40 \"C\""]
["TECHNIK","PA 1/3.40 \"D\""]
["TECHNIK","PA 1/3.40 \"E\""]
["TECHNIK","PA 1/3.40 \"F\""]
["TECHNIK","PA 1/3.40 \"G\""]
["TECHNIK","PA 1/3.40 \"H\""]
["TECHNIK","PA 1/3.40 \"I\""]
["TECHNIK","PA 1/3.40 \"J\""]
["TECHNIK","PA 1/3.40 \"K\""]
["TECHNIK","PA 1/3.40 \"L\""]
["TECHNIK","PA 1/3.40 \"l\" malé L"]
["TECHNIK","PA 1/3.40 \"M\""]
["TECHNIK","PA 1/3.40 \"N\""]
["TECHNIK","PA 1/3.40 \"N\" 1000"]
["TECHNIK","PA 1/3.40 \"P\""]
["TECHNIK","PA 1/3.40 \"Q\""]
["TECHNIK","PA 1/3.40 \"R\""]
["TECHNIK","PA 1/3.40 \"S\""]
["TECHNIK","PA 1/3.40 \"T\""]
["TECHNIK","PA 1/3.40 \"U\""]
["TECHNIK","PA 1/3.40 \"U\" 1000"]
["TECHNIK","PA 1/3.40 \"V\""]
["TECHNIK","PA 1/3.40 \"V\" 1000"]
["TECHNIK","PA 1/3.40 \"W\""]
["TECHNIK","PA 1/3.40 \"W\" 1000"]
["TECHNIK","PA 1/3.40 \"X\""]
["TECHNIK","PA 1/3.40 \"Y\""]
["TECHNIK","PA 1/3.40 \"Z\""]
["TECHNIK","PA 1/3.40 \"zem\""]
["TECHNIK","PA 1/3.40 \"zem\" 1000"]
["TECHNIK","PA 1/3.59 \"5\"euro"]
["TECHNIK","PA 1/3.6 modrá"]
["TECHNIK","PA 1/3.69 \"-\""]
["TECHNIK","PA 1/3.69 \"-\" 1000"]
["TECHNIK","PA 1/3.69 \"0\""]
["TECHNIK","PA 1/3.69 \"1\""]
["TECHNIK","PA 1/3.69 \"2\""]
["TECHNIK","PA 1/3.69 \"3\""]
["TECHNIK","PA 1/3.69 \"4\""]
["TECHNIK","PA 1/3.69 \"5\""]
["TECHNIK","PA 1/3.69 \"6\"euro"]
["TECHNIK","PA 1/3.69 \"7\""]
["TECHNIK","PA 1/3.69 \"8\""]
["TECHNIK","PA 1/3.69 \"9\""]
["TECHNIK","PA 1/3.79 \"7\"euro"]
["TECHNIK","PA 1/3.8 šedá"]
["TECHNIK","PA 1/3.80 \"8\"euro"]
["TECHNIK","PA 1/3.90 \"1\""]
["TECHNIK","PA 1/3.90 \"2\""]
["TECHNIK","PA 1/3.90 \"3\""]
["TECHNIK","PA 1/3.90 \"4\""]
["TECHNIK","PA 1/3.90 \"5\""]
["TECHNIK","PA 1/3.90 \"6\""]
["TECHNIK","PA 1/3.90 \"7\""]
["TECHNIK","PA 1/3.90 \"8\""]
["TECHNIK","PA 1/3.90 \"9\"euro"]
["TECHNIK","PA 1/6"]
["TECHNIK","PA 1/6.40 \"L1\""]
["TECHNIK","PA 1/6.40 \"L1\" 1000"]
["TECHNIK","PA 1/6.40 \"L2\""]
["TECHNIK","PA 1/6.40 \"L2\" 1000"]
["TECHNIK","PA 1/6.40 \"L3\""]
["TECHNIK","PA 1/6.40 \"L3\" 1000"]
["TECHNIK","PA 1/6.40 \"MP\""]
["TECHNIK","PA 1/6.40 \"PE\""]
["TECHNIK","PA 1/6.40 \"U1\""]
["TECHNIK","PA 1/6.40 \"U2\""]
["TECHNIK","PA 1/6.40 \"V1\""]
["TECHNIK","PA 1/6.40 \"V2\""]
["TECHNIK","PA 1/6.40 \"W1\""]
["TECHNIK","PA 1/6.40 \"W2\""]
["TECHNIK SPECIAL - AKCIA","PA 10-C"]
["TECHNIK","PA 2/12"]
["TECHNIK","PA 2/4"]
["TECHNIK","PA 2/4.19 \"1\"euro"]
["TECHNIK","PA 2/4.29 \"0\""]
["TECHNIK","PA 2/4.29 \"1\""]
["TECHNIK","PA 2/4.29 \"2\"euro"]
["TECHNIK","PA 2/4.29 \"3\""]
["TECHNIK","PA 2/4.29 \"4\""]
["TECHNIK","PA 2/4.29 \"5\""]
["TECHNIK","PA 2/4.29 \"6\""]
["TECHNIK","PA 2/4.29 \"7\""]
["TECHNIK","PA 2/4.29 \"8\""]
["TECHNIK","PA 2/4.29 \"9\""]
["TECHNIK","PA 2/4.40 \"+\""]
["TECHNIK","PA 2/4.40 \"0\""]
["TECHNIK","PA 2/4.40 \"0\" 250"]
["TECHNIK","PA 2/4.40 \"1\""]
["TECHNIK","PA 2/4.40 \"1\" 250"]
["TECHNIK","PA 2/4.40 \"2\""]
["TECHNIK","PA 2/4.40 \"2\" 250"]
["TECHNIK","PA 2/4.40 \"3\""]
["TECHNIK","PA 2/4.40 \"3\" 250"]
["TECHNIK","PA 2/4.40 \"4\"euro"]
["TECHNIK","PA 2/4.40 \"4\"euro250"]
["TECHNIK","PA 2/4.40 \"5\""]
["TECHNIK","PA 2/4.40 \"5\" 250"]
["TECHNIK","PA 2/4.40 \"6\""]
["TECHNIK","PA 2/4.40 \"6\" 250"]
["TECHNIK","PA 2/4.40 \"7\""]
["TECHNIK","PA 2/4.40 \"7\" 250"]
["TECHNIK","PA 2/4.40 \"8\""]
["TECHNIK","PA 2/4.40 \"8\" 250"]
["TECHNIK","PA 2/4.40 \"9\""]
["TECHNIK","PA 2/4.40 \"9\" 250"]
["TECHNIK","PA 2/4.40 \"A\""]
["TECHNIK","PA 2/4.40 \"B\""]
["TECHNIK","PA 2/4.40 \"C\""]
["TECHNIK","PA 2/4.40 \"D\""]
["TECHNIK","PA 2/4.40 \"E\""]
["TECHNIK","PA 2/4.40 \"F\""]
["TECHNIK","PA 2/4.40 \"G\""]
["TECHNIK","PA 2/4.40 \"H\""]
["TECHNIK","PA 2/4.40 \"I\""]
["TECHNIK","PA 2/4.40 \"J\""]
["TECHNIK","PA 2/4.40 \"K\""]
["TECHNIK","PA 2/4.40 \"L\""]
["TECHNIK","PA 2/4.40 \"M\""]
["TECHNIK","PA 2/4.40 \"N\""]
["TECHNIK","PA 2/4.40 \"O\""]
["TECHNIK","PA 2/4.40 \"P\""]
["TECHNIK","PA 2/4.40 \"Q\""]
["TECHNIK","PA 2/4.40 \"R\""]
["TECHNIK","PA 2/4.40 \"S\""]
["TECHNIK","PA 2/4.40 \"T\""]
["TECHNIK","PA 2/4.40 \"U\""]
["TECHNIK","PA 2/4.40 \"V\""]
["TECHNIK","PA 2/4.40 \"W\""]
["TECHNIK","PA 2/4.40 \"X\""]
["TECHNIK","PA 2/4.40 \"Y\""]
["TECHNIK","PA 2/4.40 \"Z\""]
["TECHNIK","PA 2/4.40 \"zem\""]
["TECHNIK","PA 2/6"]
["TECHNIK","PA 2/6.40 \"L1\""]
["TECHNIK","PA 2/6.40 \"L2\""]
["TECHNIK","PA 2/6.40 \"L3\""]
["TECHNIK","PA 2/6.40 \"W1\""]
["TECHNIK","PA 2/9.40 \"XY\""]
["TECHNIK SPECIAL - AKCIA","PA 24-C"]
["TECHNIK","PA 3/15"]
["TECHNIK","PA 3/18"]
["TECHNIK","PA 3/6"]
["TECHNIK","PA 3/6.40 \"0\""]
["TECHNIK","PA 3/6.40 \"1\""]
["TECHNIK","PA 3/6.40 \"2\""]
["TECHNIK","PA 3/6.40 \"3\""]
["TECHNIK","PA 3/6.40 \"4\""]
["TECHNIK","PA 3/6.40 \"5\""]
["TECHNIK","PA 3/6.40 \"6\""]
["TECHNIK","PA 3/6.40 \"7\""]
["TECHNIK","PA 3/6.40 \"8\""]
["TECHNIK","PA 3/6.40 \"9\""]
["TECHNIK","PA 3/6.40 \"D\""]
["TECHNIK","PA 3/6.40 \"E\""]
["TECHNIK","PA 3/6.40 \"H\""]
["TECHNIK","PA 3/6.40 \"L\""]
["TECHNIK","PA 3/6.40 \"L1\""]
["TECHNIK","PA 3/6.40 \"L2\""]
["TECHNIK","PA 3/6.40 \"L3\""]
["TECHNIK","PA 3/6.40 \"P\""]
["TECHNIK","PA 3/6.40 \"PE\""]
["TECHNIK","PA 3/6.40 \"R\""]
["TECHNIK","PA 3/6.40 \"U\""]
["TECHNIK","PA 3/6.40 \"V\""]
["TECHNIK","PA 3/6.40 \"W\""]
["TECHNIK SPECIAL - AKCIA","PA 48-C"]
["TECHNIK SPECIAL - AKCIA","PA 60-C"]
["REIKU-B","PA connector NW 07 with seal"]
["REIKU-B","PA connector NW 07 without seal"]
["REIKU-B","PA connector NW 10 with seal"]
["REIKU-B","PA connector NW 10 without seal"]
["REIKU-B","PA connector NW 12 with seal"]
["REIKU-B","PA connector NW 12 without seal"]
["REIKU-B","PA connector NW 17 with seal"]
["REIKU-B","PA connector NW 17 without seal"]
["REIKU-B","PAABB-12F"]
["REIKU-B","PAABB-17F"]
["REIKU-B","PAABB-23F"]
["REIKU-B","PAABB-29F"]
["REIKU-B","PAABB-36G"]
["REIKU-B","PAABB-48G"]
["REIKU-B","PAAOB-07M101"]
["REIKU-B","PAAOB-07M16"]
["REIKU-B","PAAOB-07M20"]
["REIKU-B","PAAOB-07P07"]
["REIKU-B","PAAOB-07P09"]
["REIKU-B","PAAOB-07P11"]
["REIKU-B","PAAOB-07P13"]
["REIKU-B","PAAOB-07P16"]
["REIKU-B","PAAOB-10P09"]
["REIKU-B","PAAOB-12P11"]
["REIKU-B","PAAOB-17P16"]
["REIKU-B","PAAOB-23P21"]
["REIKU-B","PAAOB-29P29"]
["REIKU-G","PAAOG-07M101"]
["REIKU-G","PAAOG-07M16"]
["REIKU-G","PAAOG-07M20"]
["REIKU-G","PAAOG-07P07"]
["REIKU-G","PAAOG-07P09"]
["REIKU-G","PAAOG-07P11"]
["REIKU-G","PAAOG-10P09"]
["REIKU-G","PAAOG-12P11"]
["REIKU-G","PAAOG-17P16"]
["REIKU-G","PAAOG-23P21"]
["REIKU-G","PAAOG-29P29"]
["REIKU-B","PAAVB-07P07"]
["REIKU-B","PAAVB-07P09"]
["REIKU-B","PAAVB-10P09"]
["REIKU-B","PAAVB-12P11"]
["REIKU-B","PAAVB-17P16"]
["REIKU-B","PAAVB-23P21"]
["REIKU-B","PAAVB-29P29"]
["REIKU-G","PAAVG-07P07"]
["REIKU-G","PAAVG-07P09"]
["REIKU-G","PAAVG-10P09"]
["REIKU-G","PAAVG-12P11"]
["REIKU-G","PAAVG-17P16"]
["REIKU-G","PAAVG-23P21"]
["REIKU-G","PAAVG-29P29"]
["REIKU-B","PABSG-M12"]
["REIKU-B","PABSG-M16"]
["REIKU-B","PABSG-M20"]
["REIKU-B","PABSG-M25"]
["REIKU-B","PABSG-M32"]
["REIKU-B","PABSG-M40"]
["REIKU-B","PABSG-M50"]
["REIKU-B","PABSG-M63"]
["REIKU-B","PABSG-P07"]
["REIKU-B","PABSG-P09"]
["REIKU-B","PABSG-P11"]
["REIKU-B","PABSG-P13"]
["REIKU-B","PABSG-P16"]
["REIKU-B","PABSG-P21"]
["REIKU-B","PABSG-P29"]
["REIKU-B","PABSG-P36"]
["REIKU-B","PABSG-P48"]
["REIKU-B","PACSB"]
["REIKU-G","PACSG"]
["TECHNIK","PAD-3M"]
["TECHNIK","PAD-4M"]
["REIKU-B","PADFB-42"]
["REIKU-B","PADFB-52"]
["REIKU-B","PADFB-70"]
["REIKU-B","PADGB-70"]
["REIKU-B","PADMB-70"]
["REIKU-B","PADPB-36G"]
["REIKU-B","PADPB-52"]
["REIKU-B","PADPB-68"]
["REIKU-B","PADPB-70"]
["REIKU-B","PADSB-07/10"]
["REIKU-B","PADSB-12"]
["REIKU-B","PADSB-14/17"]
["REIKU-B","PADSB-23"]
["REIKU-B","PADSB-29"]
["REIKU-B","PADSB-36"]
["REIKU-B","PADSB-48"]
["REIKU-G","PADSG-07/10"]
["REIKU-G","PADSG-12"]
["REIKU-G","PADSG-14/17"]
["REIKU-G","PADSG-23"]
["REIKU-G","PADSG-29"]
["REIKU-G","PADSG-36"]
["REIKU-G","PADSG-48"]
["REIKU-B","PAEBB-70"]
["REIKU-B","PAFHB-70"]
["REIKU-B","PAFKB-52"]
["REIKU-B","PAFKB-70"]
["REIKU-B","PAFOB-07"]
["REIKU-B","PAFOB-10"]
["REIKU-B","PAFOB-12"]
["REIKU-B","PAFOB-17"]
["REIKU-B","PAFOB-23"]
["REIKU-B","PAFOB-29"]
["REIKU-B","PAFOB-36"]
["REIKU-B","PAFOB-48"]
["REIKU-G","PAFOG-07"]
["REIKU-G","PAFOG-10"]
["REIKU-G","PAFOG-12"]
["REIKU-G","PAFOG-17"]
["REIKU-G","PAFOG-23"]
["REIKU-G","PAFOG-29"]
["REIKU-G","PAFOG-36"]
["REIKU-G","PAFOG-48"]
["REIKU-B","PAFTB-70"]
["REIKU-B","PAFVB-17"]
["REIKU-B","PAFVB-23"]
["REIKU-B","PAFVB-29"]
["REIKU-B","PAFVB-36"]
["REIKU-B","PAFVB-48"]
["REIKU-G","PAFVG-17"]
["REIKU-G","PAFVG-23"]
["REIKU-G","PAFVG-29"]
["REIKU-G","PAFVG-36"]
["REIKU-G","PAFVG-48"]
["REIKU-B","PAGGB-68i"]
["REIKU-B","PAGGB-70"]
["REIKU-B","PAGGB-70i"]
["REIKU-B","PAGHB-48"]
["REIKU-B","PAGLB-36 "]
["REIKU-B","PAGLB-48 "]
["REIKU-B","PAGLB-52"]
["REIKU-B","PAGLB-70"]
["REIKU-B","PAGLB-70L"]
["REIKU-G","PAGMB-07S22"]
["REIKU-G","PAGMB-11S22"]
["REIKU-G","PAGMB-20S32"]
["REIKU-G","PAGMB-25S32"]
["REIKU-G","PAGMB-32S40"]
["REIKU-G","PAGMB-M12"]
["REIKU-G","PAGMB-M16"]
["REIKU-G","PAGMB-M20"]
["REIKU-G","PAGMB-M25"]
["REIKU-G","PAGMB-M32"]
["REIKU-G","PAGMB-M40"]
["REIKU-G","PAGMB-M50"]
["REIKU-G","PAGMB-M63"]
["REIKU-B","PAGMG-07S22"]
["REIKU-B","PAGMG-11S22"]
["REIKU-B","PAGMG-20S32"]
["REIKU-B","PAGMG-25S32"]
["REIKU-B","PAGMG-32S40"]
["REIKU-B","PAGMG-M12"]
["REIKU-B","PAGMG-M16"]
["REIKU-B","PAGMG-M20"]
["REIKU-B","PAGMG-M25"]
["REIKU-B","PAGMG-M32"]
["REIKU-B","PAGMG-M40"]
["REIKU-B","PAGMG-M50"]
["REIKU-B","PAGMG-M63"]
["REIKU-B","PAGMG-P07"]
["REIKU-B","PAGMG-P09"]
["REIKU-B","PAGMG-P11"]
["REIKU-B","PAGMG-P13"]
["REIKU-B","PAGMG-P16"]
["REIKU-B","PAGMG-P21"]
["REIKU-B","PAGMG-P29"]
["REIKU-B","PAGMG-P36"]
["REIKU-B","PAGMG-P42"]
["REIKU-B","PAGMG-P48"]
["REIKU-B","PAGOB-07G00"]
["REIKU-B","PAGOB-07M101"]
["REIKU-B","PAGOB-07M12"]
["REIKU-B","PAGOB-07M12Z"]
["REIKU-B","PAGOB-07M16"]
["REIKU-B","PAGOB-07M20"]
["REIKU-B","PAGOB-07P07"]
["REIKU-B","PAGOB-07P07Z"]
["REIKU-B","PAGOB-07P09"]
["REIKU-B","PAGOB-07P11"]
["REIKU-B","PAGOB-07P13"]
["REIKU-B","PAGOB-07S13"]
["REIKU-B","PAGOB-10M12"]
["REIKU-B","PAGOB-10M16"]
["REIKU-B","PAGOB-10M16Z"]
["REIKU-B","PAGOB-10M20"]
["REIKU-B","PAGOB-10P07"]
["REIKU-B","PAGOB-10P09"]
["REIKU-B","PAGOB-10P09Z"]
["REIKU-B","PAGOB-10P11"]
["REIKU-B","PAGOB-10P13"]
["REIKU-B","PAGOB-10S15"]
["REIKU-B","PAGOB-12M16"]
["REIKU-B","PAGOB-12M16Z"]
["REIKU-B","PAGOB-12M20"]
["REIKU-B","PAGOB-12M20Z"]
["REIKU-B","PAGOB-12P09"]
["REIKU-B","PAGOB-12P11"]
["REIKU-B","PAGOB-12P11Z"]
["REIKU-B","PAGOB-12P13"]
["REIKU-B","PAGOB-12P13Z"]
["REIKU-B","PAGOB-12S19"]
["REIKU-B","PAGOB-17M20"]
["REIKU-B","PAGOB-17M20Z"]
["REIKU-B","PAGOB-17M25"]
["REIKU-B","PAGOB-17M32"]
["REIKU-B","PAGOB-17P11"]
["REIKU-B","PAGOB-17P13"]
["REIKU-B","PAGOB-17P16"]
["REIKU-B","PAGOB-17P16Z"]
["REIKU-B","PAGOB-17P21"]
["REIKU-B","PAGOB-17S22"]
["REIKU-B","PAGOB-23M25"]
["REIKU-B","PAGOB-23M25Z"]
["REIKU-B","PAGOB-23M32"]
["REIKU-B","PAGOB-23P16"]
["REIKU-B","PAGOB-23P21"]
["REIKU-B","PAGOB-23P21Z"]
["REIKU-B","PAGOB-23S28"]
["REIKU-B","PAGOB-23S32"]
["REIKU-B","PAGOB-29M32"]
["REIKU-B","PAGOB-29M32Z"]
["REIKU-B","PAGOB-29M40"]
["REIKU-B","PAGOB-29P29"]
["REIKU-B","PAGOB-29P29Z"]
["REIKU-B","PAGOB-29S37"]
["REIKU-B","PAGOB-29S40"]
["REIKU-B","PAGOB-36M40"]
["REIKU-B","PAGOB-36M40Z"]
["REIKU-B","PAGOB-36M50"]
["REIKU-B","PAGOB-36P29"]
["REIKU-B","PAGOB-36P36"]
["REIKU-B","PAGOB-36P36Z"]
["REIKU-B","PAGOB-42"]
["REIKU-B","PAGOB-48M50"]
["REIKU-B","PAGOB-48M63"]
["REIKU-B","PAGOB-48M63Z"]
["REIKU-B","PAGOB-48P42"]
["REIKU-B","PAGOB-48P48"]
["REIKU-B","PAGOB-48P48Z"]
["REIKU-B","PAGOB-52"]
["REIKU-B","PAGOB-70"]
["REIKU-B","PAGOB-95"]
["REIKU-G","PAGOG-07G00"]
["REIKU-G","PAGOG-07M101"]
["REIKU-G","PAGOG-07M12"]
["REIKU-G","PAGOG-07M12Z"]
["REIKU-G","PAGOG-07M16"]
["REIKU-G","PAGOG-07M20"]
["REIKU-G","PAGOG-07P07"]
["REIKU-G","PAGOG-07P07Z"]
["REIKU-G","PAGOG-07P09"]
["REIKU-G","PAGOG-07P11"]
["REIKU-G","PAGOG-07P13"]
["REIKU-G","PAGOG-07S13"]
["REIKU-G","PAGOG-10M12"]
["REIKU-G","PAGOG-10M16"]
["REIKU-G","PAGOG-10M16Z"]
["REIKU-G","PAGOG-10M20"]
["REIKU-G","PAGOG-10P07"]
["REIKU-G","PAGOG-10P09"]
["REIKU-G","PAGOG-10P09Z"]
["REIKU-G","PAGOG-10P11"]
["REIKU-G","PAGOG-10P13"]
["REIKU-G","PAGOG-10S15"]
["REIKU-G","PAGOG-12M16"]
["REIKU-G","PAGOG-12M16Z"]
["REIKU-G","PAGOG-12M20"]
["REIKU-G","PAGOG-12M20Z"]
["REIKU-G","PAGOG-12P09"]
["REIKU-G","PAGOG-12P11"]
["REIKU-G","PAGOG-12P11Z"]
["REIKU-G","PAGOG-12P13"]
["REIKU-G","PAGOG-12P13Z"]
["REIKU-G","PAGOG-12S19"]
["REIKU-G","PAGOG-17M20"]
["REIKU-G","PAGOG-17M20Z"]
["REIKU-G","PAGOG-17M25"]
["REIKU-G","PAGOG-17M32"]
["REIKU-G","PAGOG-17P11"]
["REIKU-G","PAGOG-17P13"]
["REIKU-G","PAGOG-17P16"]
["REIKU-G","PAGOG-17P16Z"]
["REIKU-G","PAGOG-17P21"]
["REIKU-G","PAGOG-17S22"]
["REIKU-G","PAGOG-23M25"]
["REIKU-G","PAGOG-23M25Z"]
["REIKU-G","PAGOG-23M32"]
["REIKU-G","PAGOG-23P16"]
["REIKU-G","PAGOG-23P21"]
["REIKU-G","PAGOG-23P21Z"]
["REIKU-G","PAGOG-23S28"]
["REIKU-G","PAGOG-23S32"]
["REIKU-G","PAGOG-29M32"]
["REIKU-G","PAGOG-29M32Z"]
["REIKU-G","PAGOG-29M40"]
["REIKU-G","PAGOG-29P29"]
["REIKU-G","PAGOG-29P29Z"]
["REIKU-G","PAGOG-29S37"]
["REIKU-G","PAGOG-29S40"]
["REIKU-G","PAGOG-36M40"]
["REIKU-G","PAGOG-36M40Z"]
["REIKU-G","PAGOG-36M50"]
["REIKU-G","PAGOG-36P29"]
["REIKU-G","PAGOG-36P36"]
["REIKU-G","PAGOG-36P36Z"]
["REIKU-G","PAGOG-48M50"]
["REIKU-G","PAGOG-48M63"]
["REIKU-G","PAGOG-48M63Z"]
["REIKU-G","PAGOG-48P42"]
["REIKU-G","PAGOG-48P48"]
["REIKU-G","PAGOG-48P48Z"]
["REIKU-G","PAGOG-52"]
["REIKU-G","PAGOG-70"]
["REIKU-G","PAGOG-95"]
["REIKU-B","PAGPB-52"]
["REIKU-B","PAGVB-07M101"]
["REIKU-B","PAGVB-07M12"]
["REIKU-B","PAGVB-07M12Z"]
["REIKU-B","PAGVB-07M16"]
["REIKU-B","PAGVB-07M20"]
["REIKU-B","PAGVB-07P07"]
["REIKU-B","PAGVB-07P07Z"]
["REIKU-B","PAGVB-07P09"]
["REIKU-B","PAGVB-07P11"]
["REIKU-B","PAGVB-07P13"]
["REIKU-B","PAGVB-10M12"]
["REIKU-B","PAGVB-10M16"]
["REIKU-B","PAGVB-10M16Z"]
["REIKU-B","PAGVB-10M20"]
["REIKU-B","PAGVB-10P07"]
["REIKU-B","PAGVB-10P09"]
["REIKU-B","PAGVB-10P09Z"]
["REIKU-B","PAGVB-10P11"]
["REIKU-B","PAGVB-10P13"]
["REIKU-B","PAGVB-12M16"]
["REIKU-B","PAGVB-12M16Z"]
["REIKU-B","PAGVB-12M20"]
["REIKU-B","PAGVB-12M20Z"]
["REIKU-B","PAGVB-12P09"]
["REIKU-B","PAGVB-12P11"]
["REIKU-B","PAGVB-12P11Z"]
["REIKU-B","PAGVB-12P13"]
["REIKU-B","PAGVB-12P13Z"]
["REIKU-B","PAGVB-17M20"]
["REIKU-B","PAGVB-17M20Z"]
["REIKU-B","PAGVB-17M25"]
["REIKU-B","PAGVB-17M32"]
["REIKU-B","PAGVB-17P11"]
["REIKU-B","PAGVB-17P13"]
["REIKU-B","PAGVB-17P16"]
["REIKU-B","PAGVB-17P16Z"]
["REIKU-B","PAGVB-17P21"]
["REIKU-B","PAGVB-23M25"]
["REIKU-B","PAGVB-23M25Z"]
["REIKU-B","PAGVB-23M32"]
["REIKU-B","PAGVB-23P16"]
["REIKU-B","PAGVB-23P21"]
["REIKU-B","PAGVB-23P21Z"]
["REIKU-B","PAGVB-29M32"]
["REIKU-B","PAGVB-29M32Z"]
["REIKU-B","PAGVB-29M40"]
["REIKU-B","PAGVB-29P29"]
["REIKU-B","PAGVB-29P29Z"]
["REIKU-B","PAGVB-36M40"]
["REIKU-B","PAGVB-36M40Z"]
["REIKU-B","PAGVB-36M50"]
["REIKU-B","PAGVB-36P29"]
["REIKU-B","PAGVB-36P36"]
["REIKU-B","PAGVB-36P36Z"]
["REIKU-B","PAGVB-48M50"]
["REIKU-B","PAGVB-48M63"]
["REIKU-B","PAGVB-48M63Z"]
["REIKU-B","PAGVB-48P42"]
["REIKU-B","PAGVB-48P48"]
["REIKU-B","PAGVB-48P48Z"]
["REIKU-G","PAGVG-07M101"]
["REIKU-G","PAGVG-07M12"]
["REIKU-G","PAGVG-07M12Z"]
["REIKU-G","PAGVG-07M16"]
["REIKU-G","PAGVG-07M20"]
["REIKU-G","PAGVG-07P07"]
["REIKU-G","PAGVG-07P07Z"]
["REIKU-G","PAGVG-07P09"]
["REIKU-G","PAGVG-07P11"]
["REIKU-G","PAGVG-07P13"]
["REIKU-G","PAGVG-10M12"]
["REIKU-G","PAGVG-10M16"]
["REIKU-G","PAGVG-10M16Z"]
["REIKU-G","PAGVG-10M20"]
["REIKU-G","PAGVG-10P07"]
["REIKU-G","PAGVG-10P09"]
["REIKU-G","PAGVG-10P09Z"]
["REIKU-G","PAGVG-10P11"]
["REIKU-G","PAGVG-10P13"]
["REIKU-G","PAGVG-12M16"]
["REIKU-G","PAGVG-12M16Z"]
["REIKU-G","PAGVG-12M20"]
["REIKU-G","PAGVG-12M20Z"]
["REIKU-G","PAGVG-12P09"]
["REIKU-G","PAGVG-12P11"]
["REIKU-G","PAGVG-12P11Z"]
["REIKU-G","PAGVG-12P13"]
["REIKU-G","PAGVG-12P13Z"]
["REIKU-G","PAGVG-17M20"]
["REIKU-G","PAGVG-17M20Z"]
["REIKU-G","PAGVG-17M25"]
["REIKU-G","PAGVG-17M32"]
["REIKU-G","PAGVG-17P11"]
["REIKU-G","PAGVG-17P13"]
["REIKU-G","PAGVG-17P16"]
["REIKU-G","PAGVG-17P16Z"]
["REIKU-G","PAGVG-17P21"]
["REIKU-G","PAGVG-23M25"]
["REIKU-G","PAGVG-23M25Z"]
["REIKU-G","PAGVG-23M32"]
["REIKU-G","PAGVG-23P16"]
["REIKU-G","PAGVG-23P21"]
["REIKU-G","PAGVG-23P21Z"]
["REIKU-G","PAGVG-29M32"]
["REIKU-G","PAGVG-29M32Z"]
["REIKU-G","PAGVG-29M40"]
["REIKU-G","PAGVG-29P29"]
["REIKU-G","PAGVG-29P29Z"]
["REIKU-G","PAGVG-36M40"]
["REIKU-G","PAGVG-36M40Z"]
["REIKU-G","PAGVG-36M50"]
["REIKU-G","PAGVG-36P29"]
["REIKU-G","PAGVG-36P36"]
["REIKU-G","PAGVG-36P36Z"]
["REIKU-G","PAGVG-48M50"]
["REIKU-G","PAGVG-48M63"]
["REIKU-G","PAGVG-48M63Z"]
["REIKU-G","PAGVG-48P42"]
["REIKU-G","PAGVG-48P48"]
["REIKU-G","PAGVG-48P48Z"]
["REIKU-B","PAHDB-07"]
["REIKU-B","PAHDB-10"]
["REIKU-B","PAHDB-12"]
["REIKU-B","PAHDB-14"]
["REIKU-B","PAHDB-17"]
["REIKU-B","PAHDB-23"]
["REIKU-B","PAHDB-29"]
["REIKU-B","PAHDB-36"]
["REIKU-B","PAHDB-48"]
["REIKU-G","PAHDG-07"]
["REIKU-G","PAHDG-10"]
["REIKU-G","PAHDG-12"]
["REIKU-G","PAHDG-14"]
["REIKU-G","PAHDG-17"]
["REIKU-G","PAHDG-23"]
["REIKU-G","PAHDG-29"]
["REIKU-G","PAHDG-36"]
["REIKU-G","PAHDG-48"]
["REIKU-B","PAHOB-07"]
["REIKU-B","PAHOB-10"]
["REIKU-B","PAHOB-12"]
["REIKU-B","PAHOB-14"]
["REIKU-B","PAHOB-17"]
["REIKU-B","PAHOB-17S"]
["REIKU-B","PAHOB-23"]
["REIKU-B","PAHOB-23S"]
["REIKU-B","PAHOB-29"]
["REIKU-B","PAHOB-29S"]
["REIKU-B","PAHOB-36"]
["REIKU-B","PAHOB-36S"]
["REIKU-B","PAHOB-36V"]
["REIKU-B","PAHOB-48"]
["REIKU-B","PAHOB-48S"]
["REIKU-B","PAHOB-48V"]
["REIKU-G","PAHOG-07"]
["REIKU-G","PAHOG-10"]
["REIKU-G","PAHOG-12"]
["REIKU-G","PAHOG-14"]
["REIKU-G","PAHOG-17"]
["REIKU-G","PAHOG-17S"]
["REIKU-G","PAHOG-23"]
["REIKU-G","PAHOG-23S"]
["REIKU-G","PAHOG-29"]
["REIKU-G","PAHOG-29S"]
["REIKU-G","PAHOG-36"]
["REIKU-G","PAHOG-36S"]
["REIKU-G","PAHOG-36V"]
["REIKU-G","PAHOG-48"]
["REIKU-G","PAHOG-48S"]
["REIKU-G","PAHOG-48V"]
["REIKU-B","PAIOB-07M081"]
["REIKU-B","PAIOB-07M121"]
["REIKU-B","PAIOB-07M16"]
["REIKU-B","PAIOB-07P07"]
["REIKU-B","PAIOB-07U05"]
["REIKU-B","PAIOB-10M121"]
["REIKU-B","PAIOB-10M16"]
["REIKU-B","PAIOB-10M181"]
["REIKU-B","PAIOB-10P07"]
["REIKU-B","PAIOB-10P09"]
["REIKU-B","PAIOB-10U05"]
["REIKU-B","PAIOB-10U07"]
["REIKU-B","PAIOB-12M16"]
["REIKU-B","PAIOB-12M20"]
["REIKU-B","PAIOB-12P11"]
["REIKU-B","PAIOB-12P13"]
["REIKU-B","PAIOB-12U05"]
["REIKU-B","PAIOB-12U06"]
["REIKU-B","PAIOB-12U07"]
["REIKU-B","PAIOB-12U09"]
["REIKU-B","PAIOB-12U10"]
["REIKU-B","PAIOB-17M20"]
["REIKU-B","PAIOB-17P13"]
["REIKU-B","PAIOB-17P16"]
["REIKU-B","PAIOB-17U07"]
["REIKU-B","PAIOB-17U09"]
["REIKU-B","PAIOB-17U10"]
["REIKU-B","PAIOB-17U11"]
["REIKU-B","PAIOB-17U14"]
["REIKU-B","PAIOB-17U17"]
["REIKU-B","PAIOB-23M25"]
["REIKU-B","PAIOB-23P21"]
["REIKU-B","PAIOB-23U14"]
["REIKU-B","PAIOB-23U17"]
["REIKU-B","PAIOB-23U18"]
["REIKU-B","PAIOB-29M32"]
["REIKU-B","PAIOB-29P29"]
["REIKU-B","PAIOB-29U24"]
["REIKU-B","PAIOB-36M40"]
["REIKU-B","PAIOB-36P36"]
["REIKU-B","PAIOB-48M50"]
["REIKU-B","PAIOB-48P48"]
["REIKU-G","PAIOG-07M081"]
["REIKU-G","PAIOG-07M121"]
["REIKU-G","PAIOG-07M16"]
["REIKU-G","PAIOG-07P07"]
["REIKU-G","PAIOG-07U05"]
["REIKU-G","PAIOG-10M121"]
["REIKU-G","PAIOG-10M16"]
["REIKU-G","PAIOG-10M181"]
["REIKU-G","PAIOG-10P07"]
["REIKU-G","PAIOG-10P09"]
["REIKU-G","PAIOG-10U05"]
["REIKU-G","PAIOG-10U07"]
["REIKU-G","PAIOG-12M16"]
["REIKU-G","PAIOG-12M20"]
["REIKU-G","PAIOG-12P11"]
["REIKU-G","PAIOG-12P13"]
["REIKU-G","PAIOG-12U05"]
["REIKU-G","PAIOG-12U06"]
["REIKU-G","PAIOG-12U07"]
["REIKU-G","PAIOG-12U09"]
["REIKU-G","PAIOG-12U10"]
["REIKU-G","PAIOG-17M20"]
["REIKU-G","PAIOG-17P13"]
["REIKU-G","PAIOG-17P16"]
["REIKU-G","PAIOG-17U07"]
["REIKU-G","PAIOG-17U09"]
["REIKU-G","PAIOG-17U10"]
["REIKU-G","PAIOG-17U11"]
["REIKU-G","PAIOG-17U14"]
["REIKU-G","PAIOG-17U17"]
["REIKU-G","PAIOG-23M25"]
["REIKU-G","PAIOG-23P21"]
["REIKU-G","PAIOG-23U14"]
["REIKU-G","PAIOG-23U17"]
["REIKU-G","PAIOG-23U18"]
["REIKU-G","PAIOG-29M32"]
["REIKU-G","PAIOG-29P29"]
["REIKU-G","PAIOG-29U24"]
["REIKU-G","PAIOG-36M40"]
["REIKU-G","PAIOG-36P36"]
["REIKU-G","PAIOG-48M50"]
["REIKU-G","PAIOG-48P48"]
["REIKU-B","PAIRB-07M081"]
["REIKU-B","PAIRB-07M121"]
["REIKU-B","PAIRB-07M16"]
["REIKU-B","PAIRB-07P07"]
["REIKU-B","PAIRB-10M121"]
["REIKU-B","PAIRB-10M16"]
["REIKU-B","PAIRB-10M181"]
["REIKU-B","PAIRB-10P07"]
["REIKU-B","PAIRB-10P09"]
["REIKU-B","PAIRB-12M16"]
["REIKU-B","PAIRB-12M20"]
["REIKU-B","PAIRB-12P11"]
["REIKU-B","PAIRB-12P13"]
["REIKU-B","PAIRB-17M20"]
["REIKU-B","PAIRB-17P13"]
["REIKU-B","PAIRB-17P16"]
["REIKU-B","PAIRB-23M25"]
["REIKU-B","PAIRB-23P21"]
["REIKU-B","PAIRB-29M32"]
["REIKU-B","PAIRB-29P29"]
["REIKU-B","PAIRB-36M40"]
["REIKU-B","PAIRB-36P36"]
["REIKU-B","PAIRB-48M50"]
["REIKU-B","PAIRB-48P48"]
["REIKU-G","PAIRG-07M081"]
["REIKU-G","PAIRG-07M121"]
["REIKU-G","PAIRG-07M16"]
["REIKU-G","PAIRG-07P07"]
["REIKU-G","PAIRG-10M121"]
["REIKU-G","PAIRG-10M16"]
["REIKU-G","PAIRG-10M181"]
["REIKU-G","PAIRG-10P07"]
["REIKU-G","PAIRG-10P09"]
["REIKU-G","PAIRG-12M16"]
["REIKU-G","PAIRG-12M20"]
["REIKU-G","PAIRG-12P11"]
["REIKU-G","PAIRG-12P13"]
["REIKU-G","PAIRG-17M20"]
["REIKU-G","PAIRG-17P13"]
["REIKU-G","PAIRG-17P16"]
["REIKU-G","PAIRG-23M25"]
["REIKU-G","PAIRG-23P21"]
["REIKU-G","PAIRG-29M32"]
["REIKU-G","PAIRG-29P29"]
["REIKU-G","PAIRG-36M40"]
["REIKU-G","PAIRG-36P36"]
["REIKU-G","PAIRG-48M50"]
["REIKU-G","PAIRG-48P48"]
["TECHNIK","Pájka s Ag"]
["TECHNIK","Pájka s Pb"]
["REIKU-B","PAKGB-36"]
["REIKU-B","PAKGB-52"]
["REIKU-B","PAKKB-70"]
["REIKU-B","PAKMB-17F/G"]
["REIKU-B","PAKMB-36/36"]
["REIKU-B","PAKMB-68"]
["REIKU-B","PAKMB-68/70"]
["REIKU-B","PAKMB-70"]
["REIKU-B","PAKMB-90"]
["REIKU-B","PAKOB-M12"]
["REIKU-B","PAKOB-M16"]
["REIKU-B","PAKOB-M20"]
["REIKU-B","PAKOB-M25"]
["REIKU-B","PAKOB-M32"]
["REIKU-B","PAKOB-M40"]
["REIKU-B","PAKOB-M50"]
["REIKU-B","PAKOB-M63"]
["REIKU-B","PAKOB-P07"]
["REIKU-B","PAKOB-P09"]
["REIKU-B","PAKOB-P11"]
["REIKU-B","PAKOB-P13"]
["REIKU-B","PAKOB-P16"]
["REIKU-B","PAKOB-P21"]
["REIKU-B","PAKOB-P29"]
["REIKU-B","PAKOB-P36"]
["REIKU-B","PAKOB-P48"]
["REIKU-G","PAKOG-M12"]
["REIKU-G","PAKOG-M16"]
["REIKU-G","PAKOG-M20"]
["REIKU-G","PAKOG-M25"]
["REIKU-G","PAKOG-M32"]
["REIKU-G","PAKOG-M40"]
["REIKU-G","PAKOG-M50"]
["REIKU-G","PAKOG-M63"]
["REIKU-G","PAKOG-P07"]
["REIKU-G","PAKOG-P09"]
["REIKU-G","PAKOG-P11"]
["REIKU-G","PAKOG-P13"]
["REIKU-G","PAKOG-P16"]
["REIKU-G","PAKOG-P21"]
["REIKU-G","PAKOG-P29"]
["REIKU-G","PAKOG-P36"]
["REIKU-G","PAKOG-P48"]
["REIKU-B","PAKPB-29"]
["REIKU-B","PAKPB-42"]
["REIKU-B","PAKTB-70"]
["REIKU-B","PAM1216"]
["REIKU-B","PAM1612"]
["REIKU-B","PAM1620"]
["REIKU-B","PAM2012"]
["REIKU-B","PAM2016"]
["REIKU-B","PAM2025"]
["REIKU-B","PAM2516"]
["REIKU-B","PAM2520"]
["REIKU-B","PAM2532"]
["REIKU-B","PAM3220"]
["REIKU-B","PAM3225"]
["REIKU-B","PAM3240"]
["REIKU-B","PAM4025"]
["REIKU-B","PAM4032"]
["REIKU-B","PAM5032"]
["REIKU-B","PAM5040"]
["REIKU-B","PAM6340"]
["REIKU-B","PAM6350"]
["REIKU-B","PAMBB-23F/G"]
["REIKU-B","PAMBB-29F/G"]
["REIKU-B","PAMBB-36F/G"]
["REIKU-B","PAMBB-42"]
["REIKU-B","PAMBB-42/36"]
["REIKU-B","PAMBB-48F/G"]
["REIKU-B","PAMBB-52"]
["REIKU-B","PAMBB-70"]
["REIKU-B","PAMBB-70L"]
["REIKU-B","PAMCN-29"]
["REIKU-B","PAMCN-36"]
["REIKU-B","PAMCN-42"]
["REIKU-B","PAMCN-52"]
["REIKU-B","PAMCN-70"]
["REIKU-G","PAMCR-29"]
["REIKU-G","PAMCR-36"]
["REIKU-G","PAMCR-42"]
["REIKU-G","PAMCR-52"]
["REIKU-G","PAMCR-70"]
["REIKU-B","PANOB-07M081"]
["REIKU-B","PANOB-07M121"]
["REIKU-B","PANOB-07M181"]
["REIKU-B","PANOB-07M301"]
["REIKU-B","PANOB-10M081"]
["REIKU-B","PANOB-10M121"]
["REIKU-B","PANOB-10M181"]
["REIKU-B","PANOB-10M301"]
["REIKU-G","PANOG-07M081"]
["REIKU-G","PANOG-07M121"]
["REIKU-G","PANOG-07M181"]
["REIKU-G","PANOG-07M301"]
["REIKU-G","PANOG-10M081"]
["REIKU-G","PANOG-10M121"]
["REIKU-G","PANOG-10M181"]
["REIKU-G","PANOG-10M301"]
["REIKU-B","PAP1109"]
["REIKU-B","PAP1113"]
["REIKU-B","PAP1309"]
["REIKU-B","PAP1311"]
["REIKU-B","PAP1316"]
["REIKU-B","PAP1609"]
["REIKU-B","PAP1611"]
["REIKU-B","PAP1613"]
["REIKU-B","PAP2113"]
["REIKU-B","PAP2116"]
["REIKU-B","PAP2921"]
["REIKU-B","PAP3629"]
["REIKU-B","PAPKB-17F/G"]
["REIKU-B","PAPKB-29F/G"]
["REIKU-B","PAPKB-36F/G"]
["REIKU-B","PAPRB-23F/G"]
["REIKU-B","PAPRB-29F/G"]
["REIKU-B","PAPRB-36F/G"]
["REIKU-B","PAPRB-42"]
["REIKU-B","PAPRB-48F/G"]
["REIKU-B","PAPRB-52"]
["REIKU-B","PAPRB-52BL"]
["REIKU-B","PAPRB-68"]
["REIKU-B","PAPRB-70"]
["REIKU-B","PAPRB-70BL"]
["REIKU-B","PAPRB-90"]
["REIKU-B","PARAB-07G"]
["REIKU-B","PARAB–10F"]
["REIKU-B","PARAB–12F"]
["REIKU-B","PARAB–17F"]
["REIKU-B","PARAB–23F"]
["REIKU-B","PARAB-23G"]
["REIKU-B","PARAB–29F"]
["REIKU-B","PARAB–29G"]
["REIKU-B","PARAB-36F"]
["REIKU-B","PARAB–36G"]
["REIKU-B","PARAB-42M"]
["REIKU-B","PARAB-48F"]
["REIKU-B","PARAB-48G"]
["REIKU-B","PARAB-52G"]
["REIKU-B","PARAB-68G"]
["REIKU-B","PARAB-70G"]
["REIKU-B","PARBB-12F"]
["REIKU-B","PARBB-17F"]
["REIKU-B","PARBB-23F"]
["REIKU-B","PARBB-29F"]
["REIKU-B","PARBB-36G"]
["REIKU-B","PARBB-48G"]
["REIKU-B","PAREB–07G"]
["REIKU-B","PAREB–10F"]
["REIKU-B","PAREB–12F"]
["REIKU-B","PAREB–14F"]
["REIKU-B","PAREB–17F"]
["REIKU-B","PAREB–23F"]
["REIKU-B","PAREB–29F"]
["REIKU-B","PAREB–36F"]
["REIKU-B","PAREB–48F"]
["REIKU-B","PAREB–52G"]
["REIKU-B","PAREB–70G"]
["REIKU-B","PAREB–95G"]
["REIKU-G","PAREG–07G"]
["REIKU-G","PAREG–10F"]
["REIKU-G","PAREG–12F"]
["REIKU-G","PAREG–14F"]
["REIKU-G","PAREG–17F"]
["REIKU-G","PAREG–23F"]
["REIKU-G","PAREG–29F"]
["REIKU-G","PAREG–36F"]
["REIKU-G","PAREG-48F"]
["REIKU-G","PAREG–52G"]
["REIKU-G","PAREG–70G"]
["REIKU-G","PAREG–95G"]
["REIKU-B","PARFB-10F"]
["REIKU-B","PARFB-12F"]
["REIKU-B","PARFB-17F"]
["REIKU-B","PARFB-17G"]
["REIKU-B","PARFB-23G"]
["REIKU-B","PARFB-29G"]
["REIKU-B","PARFB-36G"]
["REIKU-B","PARFB-48G"]
["REIKU-B","PARFB-52G"]
["REIKU-B","PARFB-70G"]
["REIKU-B","PARGB-48"]
["REIKU-B","PARGB-48L48K"]
["REIKU-B","PARGB-48L52K"]
["REIKU-B","PARGB-48R48K"]
["REIKU-B","PARGB-48R52K"]
["REIKU-B","PARGB-48T"]
["REIKU-B","PARGB-76"]
["REIKU-B","PARGB-76L70"]
["REIKU-B","PARGB-76L90"]
["REIKU-B","PARGB-76R70"]
["REIKU-B","PARGB-76R90"]
["REIKU-B","PARNB–07G"]
["REIKU-B","PARNB–10F"]
["REIKU-B","PARNB–12F"]
["REIKU-B","PARNB–14F"]
["REIKU-B","PARNB–17F"]
["REIKU-B","PARNB–17G"]
["REIKU-B","PARNB–23F"]
["REIKU-B","PARNB–23G"]
["REIKU-B","PARNB–29F"]
["REIKU-B","PARNB–29G"]
["REIKU-B","PARNB–36F"]
["REIKU-B","PARNB–36G"]
["REIKU-B","PARNB–48F"]
["REIKU-B","PARNB–48G"]
["REIKU-B","PARNB–52G"]
["REIKU-B","PARNB–70G"]
["REIKU-B","PARNB–95G"]
["REIKU-G","PARNG–07G"]
["REIKU-G","PARNG–10F"]
["REIKU-G","PARNG–12F"]
["REIKU-G","PARNG–14F"]
["REIKU-G","PARNG–17F"]
["REIKU-G","PARNG–17G"]
["REIKU-G","PARNG–23F"]
["REIKU-G","PARNG–23G"]
["REIKU-G","PARNG–29F"]
["REIKU-G","PARNG–29G"]
["REIKU-G","PARNG–36F"]
["REIKU-G","PARNG–36G"]
["REIKU-G","PARNG–48F"]
["REIKU-G","PARNG–48G"]
["REIKU-G","PARNG–52G"]
["REIKU-G","PARNG–70G"]
["REIKU-G","PARNG–95G"]
["REIKU-B","PARRB–07G"]
["REIKU-B","PARRB–10F"]
["REIKU-B","PARRB–12F"]
["REIKU-B","PARRB–17F"]
["REIKU-B","PARRB–23F"]
["REIKU-B","PARRB–23G"]
["REIKU-B","PARRB–29F"]
["REIKU-B","PARRB–29G"]
["REIKU-B","PARRB-36F"]
["REIKU-B","PARRB–36G"]
["REIKU-B","PARRB-48F"]
["REIKU-B","PARRB–48G"]
["REIKU-B","PARRB–52G"]
["REIKU-B","PARRB–70G"]
["REIKU-B","PARRB–95G"]
["REIKU-G","PARRG–07G"]
["REIKU-G","PARRG–10F"]
["REIKU-G","PARRG–12F"]
["REIKU-G","PARRG–17F"]
["REIKU-G","PARRG–23F"]
["REIKU-G","PARRG–23G"]
["REIKU-G","PARRG–29F"]
["REIKU-G","PARRG–29G"]
["REIKU-G","PARRG-36F"]
["REIKU-G","PARRG–36G"]
["REIKU-G","PARRG–48G"]
["REIKU-G","PARRG–52G"]
["REIKU-G","PARRG–70G"]
["REIKU-G","PARRG–95G"]
["REIKU-B","PARTB-10"]
["REIKU-B","PARTB-12"]
["REIKU-B","PARTB-14"]
["REIKU-B","PARTB-17"]
["REIKU-B","PARTB-24"]
["REIKU-B","PARTB-29"]
["REIKU-B","PARTB-34"]
["REIKU-B","PARTB-45"]
["REIKU-B","PARTB-68"]
["REIKU-B","PARVB–07G"]
["REIKU-B","PARVB–10F"]
["REIKU-B","PARVB–12F"]
["REIKU-B","PARVB–17F"]
["REIKU-B","PARVB–17G"]
["REIKU-B","PARVB–23F"]
["REIKU-B","PARVB–23G"]
["REIKU-B","PARVB–29F"]
["REIKU-B","PARVB–29G"]
["REIKU-B","PARVB–36G"]
["REIKU-B","PARVB–48G"]
["REIKU-B","PARVB–52G"]
["REIKU-B","PARVB–70G"]
["REIKU-B","PARVB–95G"]
["REIKU-G","PARVG–07G"]
["REIKU-G","PARVG–10F"]
["REIKU-G","PARVG–12F"]
["REIKU-G","PARVG–17F"]
["REIKU-G","PARVG–17G"]
["REIKU-G","PARVG–23F"]
["REIKU-G","PARVG–23G"]
["REIKU-G","PARVG–29G"]
["REIKU-G","PARVG–36G"]
["REIKU-G","PARVG–48G"]
["REIKU-G","PARVG–52G"]
["REIKU-G","PARVG–70G"]
["REIKU-G","PARVG–95G"]
["REIKU-B","PASOB-07M12"]
["REIKU-B","PASOB-07M16"]
["REIKU-B","PASOB-07M20"]
["REIKU-B","PASOB-07P07"]
["REIKU-B","PASOB-07P09"]
["REIKU-B","PASOB-07P11"]
["REIKU-B","PASOB-07P13"]
["REIKU-B","PASOB-17M25"]
["REIKU-B","PASOB-17P16"]
["REIKU-B","PASOB-23M32"]
["REIKU-B","PASOB-23P21"]
["REIKU-B","PASOB-52"]
["REIKU-B","PASOB-70"]
["REIKU-B","PASOB-95"]
["REIKU-G","PASOG-07M12"]
["REIKU-G","PASOG-07M16"]
["REIKU-G","PASOG-07M20"]
["REIKU-G","PASOG-07P07"]
["REIKU-G","PASOG-07P09"]
["REIKU-G","PASOG-07P11"]
["REIKU-G","PASOG-07P13"]
["REIKU-G","PASOG-17M25"]
["REIKU-G","PASOG-17P16"]
["REIKU-G","PASOG-23M32"]
["REIKU-G","PASOG-23P21"]
["REIKU-G","PASOG-52"]
["REIKU-G","PASOG-70"]
["REIKU-G","PASOG-95"]
["REIKU-B","PASSB-17K"]
["REIKU-B","PASSB-29K"]
["REIKU-B","PASSB-36K"]
["REIKU-B","PASSB-36S"]
["REIKU-B","PASSB-52K"]
["REIKU-B","PASSB-52M"]
["REIKU-B","PASSB-52S"]
["REIKU-B","PASSB-70K"]
["REIKU-B","PASSB-70M"]
["REIKU-B","PASSB-70SE"]
["TECHNIK","PASTA"]
["REIKU-B","PASVB-07M12"]
["REIKU-B","PASVB-07M16"]
["REIKU-B","PASVB-07M20"]
["REIKU-B","PASVB-07P07"]
["REIKU-B","PASVB-07P09"]
["REIKU-B","PASVB-07P11"]
["REIKU-B","PASVB-07P13"]
["REIKU-B","PASVB-17M25"]
["REIKU-B","PASVB-17P16"]
["REIKU-B","PASVB-23M32"]
["REIKU-B","PASVB-23P21"]
["REIKU-G","PASVG-07M12"]
["REIKU-G","PASVG-07M16"]
["REIKU-G","PASVG-07M20"]
["REIKU-G","PASVG-07P07"]
["REIKU-G","PASVG-07P09"]
["REIKU-G","PASVG-07P11"]
["REIKU-G","PASVG-07P13"]
["REIKU-G","PASVG-17M25"]
["REIKU-G","PASVG-17P16"]
["REIKU-G","PASVG-23M32"]
["REIKU-G","PASVG-23P21"]
["REIKU-B","PATBB-70"]
["REIKU-B","PAVGB-23"]
["REIKU-B","PAVGB-36"]
["REIKU-B","PAVGB-70"]
["REIKU-B","PAVSB"]
["REIKU-G","PAVSG"]
["REIKU-B","PAWAB-14/17"]
["REIKU-B","PAWOB-07P07"]
["REIKU-B","PAWOB-10M16"]
["REIKU-B","PAWOB-10M20"]
["REIKU-B","PAWOB-10P07"]
["REIKU-B","PAWOB-10P09"]
["REIKU-B","PAWOB-10P11"]
["REIKU-B","PAWOB-12M16"]
["REIKU-B","PAWOB-12M20"]
["REIKU-B","PAWOB-12P09"]
["REIKU-B","PAWOB-12P11"]
["REIKU-B","PAWOB-12P13"]
["REIKU-B","PAWOB-17M20"]
["REIKU-B","PAWOB-17M25"]
["REIKU-B","PAWOB-17P13"]
["REIKU-B","PAWOB-17P16"]
["REIKU-B","PAWOB-23M25"]
["REIKU-B","PAWOB-23P21"]
["REIKU-B","PAWOB-29M32"]
["REIKU-B","PAWOB-29P29"]
["REIKU-B","PAWOB-36M40"]
["REIKU-B","PAWOB-36P36"]
["REIKU-B","PAWOB-48M50"]
["REIKU-B","PAWOB-48P48"]
["REIKU-B","PAWOB-52"]
["REIKU-B","PAWOB-70"]
["REIKU-B","PAWOB-95"]
["REIKU-G","PAWOG-07P07"]
["REIKU-G","PAWOG-10M16"]
["REIKU-G","PAWOG-10M20"]
["REIKU-G","PAWOG-10P07"]
["REIKU-G","PAWOG-10P09"]
["REIKU-G","PAWOG-10P11"]
["REIKU-G","PAWOG-12M16"]
["REIKU-G","PAWOG-12M20"]
["REIKU-G","PAWOG-12P09"]
["REIKU-G","PAWOG-12P11"]
["REIKU-G","PAWOG-12P13"]
["REIKU-G","PAWOG-17M20"]
["REIKU-G","PAWOG-17M25"]
["REIKU-G","PAWOG-17P13"]
["REIKU-G","PAWOG-17P16"]
["REIKU-G","PAWOG-23M25"]
["REIKU-G","PAWOG-23P21"]
["REIKU-G","PAWOG-29M32"]
["REIKU-G","PAWOG-29P29"]
["REIKU-G","PAWOG-36M40"]
["REIKU-G","PAWOG-36P36"]
["REIKU-G","PAWOG-48M50"]
["REIKU-G","PAWOG-48P48"]
["REIKU-G","PAWOG-52"]
["REIKU-G","PAWOG-70"]
["REIKU-G","PAWOG-95"]
["REIKU-B","PAWVB-07P07"]
["REIKU-B","PAWVB-10M16"]
["REIKU-B","PAWVB-10M20"]
["REIKU-B","PAWVB-10P07"]
["REIKU-B","PAWVB-10P09"]
["REIKU-B","PAWVB-10P11"]
["REIKU-B","PAWVB-10P11K"]
["REIKU-B","PAWVB-10P13"]
["REIKU-B","PAWVB-12M16"]
["REIKU-B","PAWVB-12M20"]
["REIKU-B","PAWVB-12P09"]
["REIKU-B","PAWVB-12P11"]
["REIKU-B","PAWVB-12P13"]
["REIKU-B","PAWVB-17M20"]
["REIKU-B","PAWVB-17P13"]
["REIKU-B","PAWVB-17P16"]
["REIKU-B","PAWVB-23M25"]
["REIKU-B","PAWVB-23P21"]
["REIKU-B","PAWVB-29M32"]
["REIKU-B","PAWVB-29P29"]
["REIKU-B","PAWVB-36M40"]
["REIKU-B","PAWVB-36P36"]
["REIKU-B","PAWVB-48M50"]
["REIKU-B","PAWVB-48P48"]
["REIKU-G","PAWVG-07P07"]
["REIKU-G","PAWVG-10M16"]
["REIKU-G","PAWVG-10M20"]
["REIKU-G","PAWVG-10P07"]
["REIKU-G","PAWVG-10P09"]
["REIKU-G","PAWVG-10P11"]
["REIKU-G","PAWVG-10P11K"]
["REIKU-G","PAWVG-10P13"]
["REIKU-G","PAWVG-12M16"]
["REIKU-G","PAWVG-12M20"]
["REIKU-G","PAWVG-12P09"]
["REIKU-G","PAWVG-12P11"]
["REIKU-G","PAWVG-12P13"]
["REIKU-G","PAWVG-17M20"]
["REIKU-G","PAWVG-17P13"]
["REIKU-G","PAWVG-17P16"]
["REIKU-G","PAWVG-23M25"]
["REIKU-G","PAWVG-23P21"]
["REIKU-G","PAWVG-29M32"]
["REIKU-G","PAWVG-29P29"]
["REIKU-G","PAWVG-36M40"]
["REIKU-G","PAWVG-36P36"]
["REIKU-G","PAWVG-48M50"]
["REIKU-G","PAWVG-48P48"]
["TECHNIK","PAZ 02KN4"]
["TECHNIK","PAZ 10KN4"]
["TECHNIK","PAZ 20KN4"]
["TECHNIK","PB  8"]
["TECHNIK","PB 10"]
["TECHNIK","PB 12"]
["TECHNIK","PB 14"]
["TECHNIK","PB 2,0 bílá"]
["TECHNIK","PB 2,0 žlutá"]
["TECHNIK","PB 2,5 bílá"]
["TECHNIK","PB 2,5 žlutá"]
["TECHNIK","PB 3,0 bílá"]
["TECHNIK","PB 3,0 žlutá"]
["TECHNIK","PB 3,2 žlutá"]
["TECHNIK","PB 3,5 bílá"]
["TECHNIK","PB 3,5 žlutá"]
["TECHNIK","PB 4,0 bílá"]
["TECHNIK","PB 4,0 žlutá"]
["TECHNIK","PB 4,5 bílá"]
["TECHNIK","PB 4,5 žlutá"]
["TECHNIK","PB 5,0 bílá"]
["TECHNIK","PB 5,0 žlutá"]
["TECHNIK","PB 5,5 bílá"]
["TECHNIK","PB 5,5 žlutá"]
["TECHNIK","PB 6,0 bílá"]
["TECHNIK","PB 6,0 žlutá"]
["TECHNIK","PB 8,0 bílá"]
["TECHNIK","PB 8,0 žlutá"]
["TECHNIK","PB10,0 bílá"]
["TECHNIK","PB10,0 žlutá"]
["TECHNIK","PB175-E"]
["TECHNIK","PB340-7/16"]
["TECHNIK","PBD 300"]
["TECHNIK","PBF  1,6/0,8 bílá"]
["TECHNIK","PBF  1,6/0,8 černá"]
["TECHNIK","PBF  1,6/0,8 černá R"]
["TECHNIK","PBF  1,6/0,8 fialová"]
["TECHNIK","PBF  1,6/0,8 hnědá"]
["TECHNIK","PBF  1,6/0,8 modrá"]
["TECHNIK","PBF  1,6/0,8 oranž"]
["TECHNIK","PBF  1,6/0,8 rudá"]
["TECHNIK","PBF  1,6/0,8 transp"]
["TECHNIK","PBF  1,6/0,8 zelená"]
["TECHNIK","PBF  1,6/0,8 žlutá"]
["TECHNIK","PBF  1,6/0,8 žz"]
["TECHNIK","PBF  2,4/1,2 bílá"]
["TECHNIK","PBF  2,4/1,2 bílá R"]
["TECHNIK","PBF  2,4/1,2 bílá T"]
["TECHNIK","PBF  2,4/1,2 černá"]
["TECHNIK","PBF  2,4/1,2 černá R"]
["TECHNIK","PBF  2,4/1,2 fialová"]
["TECHNIK","PBF  2,4/1,2 hnědá"]
["TECHNIK","PBF  2,4/1,2 modrá"]
["TECHNIK","PBF  2,4/1,2 modrá R"]
["TECHNIK","PBF  2,4/1,2 oranž"]
["TECHNIK","PBF  2,4/1,2 rudá"]
["TECHNIK","PBF  2,4/1,2 transp"]
["TECHNIK","PBF  2,4/1,2 zelená"]
["TECHNIK","PBF  2,4/1,2 žlutá"]
["TECHNIK","PBF  2,4/1,2 žlutá R"]
["TECHNIK","PBF  2,4/1,2 žz"]
["TECHNIK","PBF  3,2/1,6 bílá"]
["TECHNIK","PBF  3,2/1,6 bílá R"]
["TECHNIK","PBF  3,2/1,6 bílá T"]
["TECHNIK","PBF  3,2/1,6 černá"]
["TECHNIK","PBF  3,2/1,6 černá R"]
["TECHNIK","PBF  3,2/1,6 fialová"]
["TECHNIK","PBF  3,2/1,6 hnědá"]
["TECHNIK","PBF  3,2/1,6 modrá"]
["TECHNIK","PBF  3,2/1,6 oranž"]
["TECHNIK","PBF  3,2/1,6 oranž R"]
["TECHNIK","PBF  3,2/1,6 rudá"]
["TECHNIK","PBF  3,2/1,6 šedá"]
["TECHNIK","PBF  3,2/1,6 transp"]
["TECHNIK","PBF  3,2/1,6 zelen R"]
["TECHNIK","PBF  3,2/1,6 zelená"]
["TECHNIK","PBF  3,2/1,6 žlutá"]
["TECHNIK","PBF  3,2/1,6 žlutá R"]
["TECHNIK","PBF  3,2/1,6 žz"]
["TECHNIK","PBF  4,8/2,4 bílá"]
["TECHNIK","PBF  4,8/2,4 bílá R"]
["TECHNIK","PBF  4,8/2,4 bílá T"]
["TECHNIK","PBF  4,8/2,4 černá"]
["TECHNIK","PBF  4,8/2,4 černá R"]
["TECHNIK","PBF  4,8/2,4 fialová"]
["TECHNIK","PBF  4,8/2,4 hnědá"]
["TECHNIK","PBF  4,8/2,4 modrá"]
["TECHNIK","PBF  4,8/2,4 oranž"]
["TECHNIK","PBF  4,8/2,4 oranž R"]
["TECHNIK","PBF  4,8/2,4 rudá"]
["TECHNIK","PBF  4,8/2,4 šedá"]
["TECHNIK","PBF  4,8/2,4 transp"]
["TECHNIK","PBF  4,8/2,4 zelená"]
["TECHNIK","PBF  4,8/2,4 žlutá"]
["TECHNIK","PBF  4,8/2,4 žlutá R"]
["TECHNIK","PBF  4,8/2,4 žz"]
["TECHNIK","PBF  4/1 bílá"]
["TECHNIK","PBF  4/1 bílá R"]
["TECHNIK","PBF  4/1 černá"]
["TECHNIK","PBF  4/1 fialová"]
["TECHNIK","PBF  4/1 hnědá"]
["TECHNIK","PBF  4/1 modrá"]
["TECHNIK","PBF  4/1 oranž"]
["TECHNIK","PBF  4/1 rudá"]
["TECHNIK","PBF  4/1 transp"]
["TECHNIK","PBF  4/1 zelená"]
["TECHNIK","PBF  4/1 žlutá"]
["TECHNIK","PBF  4/1 žz"]
["TECHNIK","PBF  6,4/3,2 bílá"]
["TECHNIK","PBF  6,4/3,2 bílá T"]
["TECHNIK","PBF  6,4/3,2 černá"]
["TECHNIK","PBF  6,4/3,2 černá R"]
["TECHNIK","PBF  6,4/3,2 fialová"]
["TECHNIK","PBF  6,4/3,2 hnědá"]
["TECHNIK","PBF  6,4/3,2 modrá"]
["TECHNIK","PBF  6,4/3,2 oranž"]
["TECHNIK","PBF  6,4/3,2 rudá"]
["TECHNIK","PBF  6,4/3,2 šedá"]
["TECHNIK","PBF  6,4/3,2 transp"]
["TECHNIK","PBF  6,4/3,2 zelená"]
["TECHNIK","PBF  6,4/3,2 žlutá"]
["TECHNIK","PBF  6,4/3,2 žlutá R"]
["TECHNIK","PBF  6,4/3,2 žz"]
["TECHNIK","PBF  8/2 bílá"]
["TECHNIK","PBF  8/2 bílá R"]
["TECHNIK","PBF  8/2 černá"]
["TECHNIK","PBF  8/2 černá R"]
["TECHNIK","PBF  8/2 fialová"]
["TECHNIK","PBF  8/2 hnědá"]
["TECHNIK","PBF  8/2 modrá"]
["TECHNIK","PBF  8/2 oranž"]
["TECHNIK","PBF  8/2 rudá"]
["TECHNIK","PBF  8/2 šedá"]
["TECHNIK","PBF  8/2 transp"]
["TECHNIK","PBF  8/2 zelená"]
["TECHNIK","PBF  8/2 žlutá"]
["TECHNIK","PBF  8/2 žz"]
["TECHNIK","PBF  9,5/4,8 bílá"]
["TECHNIK","PBF  9,5/4,8 černá"]
["TECHNIK","PBF  9,5/4,8 černá R"]
["TECHNIK","PBF  9,5/4,8 fialová"]
["TECHNIK","PBF  9,5/4,8 hnědá"]
["TECHNIK","PBF  9,5/4,8 modrá"]
["TECHNIK","PBF  9,5/4,8 oranž"]
["TECHNIK","PBF  9,5/4,8 oranž R"]
["TECHNIK","PBF  9,5/4,8 rudá"]
["TECHNIK","PBF  9,5/4,8 šedá"]
["TECHNIK","PBF  9,5/4,8 transp"]
["TECHNIK","PBF  9,5/4,8 zelená"]
["TECHNIK","PBF  9,5/4,8 žlutá"]
["TECHNIK","PBF  9,5/4,8 žz"]
["TECHNIK","PBF 12,7/6,4 bílá"]
["TECHNIK","PBF 12,7/6,4 černá"]
["TECHNIK","PBF 12,7/6,4 černá R"]
["TECHNIK","PBF 12,7/6,4 fialová"]
["TECHNIK","PBF 12,7/6,4 hnědá"]
["TECHNIK","PBF 12,7/6,4 modrá"]
["TECHNIK","PBF 12,7/6,4 oranž"]
["TECHNIK","PBF 12,7/6,4 oranž R"]
["TECHNIK","PBF 12,7/6,4 rudá"]
["TECHNIK","PBF 12,7/6,4 šedá"]
["TECHNIK","PBF 12,7/6,4 šedá R"]
["TECHNIK","PBF 12,7/6,4 transp"]
["TECHNIK","PBF 12,7/6,4 zelená"]
["TECHNIK","PBF 12,7/6,4 žlutá"]
["TECHNIK","PBF 12,7/6,4 žz"]
["TECHNIK","PBF 19/9,5 bílá"]
["TECHNIK","PBF 19/9,5 bílá R"]
["TECHNIK","PBF 19/9,5 černá"]
["TECHNIK","PBF 19/9,5 černá R"]
["TECHNIK","PBF 19/9,5 fialová"]
["TECHNIK","PBF 19/9,5 hnědá"]
["TECHNIK","PBF 19/9,5 modrá"]
["TECHNIK","PBF 19/9,5 modrá R"]
["TECHNIK","PBF 19/9,5 oranž"]
["TECHNIK","PBF 19/9,5 rudá"]
["TECHNIK","PBF 19/9,5 rudá R"]
["TECHNIK","PBF 19/9,5 šedá"]
["TECHNIK","PBF 19/9,5 transp"]
["TECHNIK","PBF 19/9,5 transp R"]
["TECHNIK","PBF 19/9,5 zelená"]
["TECHNIK","PBF 19/9,5 zelená R"]
["TECHNIK","PBF 19/9,5 žlutá"]
["TECHNIK","PBF 19/9,5 žlutá R"]
["TECHNIK","PBF 19/9,5 žz"]
["TECHNIK","PBF 25,4/12,7bílá"]
["TECHNIK","PBF 25,4/12,7černá"]
["TECHNIK","PBF 25,4/12,7černá R"]
["TECHNIK","PBF 25,4/12,7fialová"]
["TECHNIK","PBF 25,4/12,7hnědá"]
["TECHNIK","PBF 25,4/12,7hnědá R"]
["TECHNIK","PBF 25,4/12,7modrá"]
["TECHNIK","PBF 25,4/12,7oranž"]
["TECHNIK","PBF 25,4/12,7rudá"]
["TECHNIK","PBF 25,4/12,7šedá"]
["TECHNIK","PBF 25,4/12,7transp"]
["TECHNIK","PBF 25,4/12,7zelená"]
["TECHNIK","PBF 25,4/12,7žlutá"]
["TECHNIK","PBF 25,4/12,7žlutá R"]
["TECHNIK","PBF 25,4/12,7žz"]
["TECHNIK","PBF 31,8/15,9 černá"]
["TECHNIK","PBF 31,8/15,9 modrá"]
["TECHNIK","PBF 31,8/15,9 rudá"]
["TECHNIK","PBF 31,8/15,9 žlutá"]
["TECHNIK","PBF 31,8/15,9 žz"]
["TECHNIK","PBF 38/19 bílá"]
["TECHNIK","PBF 38/19 černá"]
["TECHNIK","PBF 38/19 fialová"]
["TECHNIK","PBF 38/19 hnědá"]
["TECHNIK","PBF 38/19 modrá"]
["TECHNIK","PBF 38/19 modrá R"]
["TECHNIK","PBF 38/19 oranž"]
["TECHNIK","PBF 38/19 rudá"]
["TECHNIK","PBF 38/19 rudá R"]
["TECHNIK","PBF 38/19 šedá"]
["TECHNIK","PBF 38/19 transp"]
["TECHNIK","PBF 38/19 zelená"]
["TECHNIK","PBF 38/19 žlutá"]
["TECHNIK","PBF 38/19 žz"]
["TECHNIK","PBF 51/25,4 bílá"]
["TECHNIK","PBF 51/25,4 černá"]
["TECHNIK","PBF 51/25,4 modrá"]
["TECHNIK","PBF 51/25,4 oranž"]
["TECHNIK","PBF 51/25,4 rudá"]
["TECHNIK","PBF 51/25,4 šedá"]
["TECHNIK","PBF 51/25,4 transp"]
["TECHNIK","PBF 51/25,4 zelená"]
["TECHNIK","PBF 51/25,4 zelená R"]
["TECHNIK","PBF 51/25,4 žlutá"]
["TECHNIK","PBF 51/25,4 žlutá R"]
["TECHNIK","PBF 51/25,4 žz"]
["TECHNIK","PBF 76/38 bílá"]
["TECHNIK","PBF 76/38 černá"]
["TECHNIK","PBF 76/38 modrá"]
["TECHNIK","PBF 76/38 modrá R"]
["TECHNIK","PBF 76/38 rudá"]
["TECHNIK","PBF 76/38 transp"]
["TECHNIK","PBF 76/38 žlutá"]
["TECHNIK","PBF 76/38 žz"]
["TECHNIK","PBF102/51 černá"]
["TECHNIK","PBF102/51 modrá"]
["TECHNIK","PBF102/51 rudá"]
["TECHNIK","PBF102/51 transp"]
["TECHNIK","PBK 10"]
["TECHNIK","PBK 12"]
["TECHNIK","PBK 14"]
["TECHNIK","PBOX černý"]
["TECHNIK","PBOX modrý"]
["TECHNIK","PBOX oranžový"]
["TECHNIK","PBOX rudý"]
["TECHNIK","PBOX sv. šedý"]
["TECHNIK","PBOX tm. šedý"]
["TECHNIK","PBOX zelený"]
["TECHNIK","PBOX žlutý"]
["TECHNIK","PBR  8"]
["TECHNIK","PBR  9"]
["TECHNIK","PBR 10"]
["TECHNIK","PBR 14"]
["TECHNIK","PC 10/12"]
["TECHNIK","PC 10/15"]
["TECHNIK","PC 10/3"]
["TECHNIK","PC 10/3 \"0\""]
["TECHNIK","PC 10/3 \"1\""]
["TECHNIK","PC 10/3 \"2\""]
["TECHNIK","PC 10/3 \"3\""]
["TECHNIK","PC 10/3 \"4\""]
["TECHNIK","PC 10/3 \"5\""]
["TECHNIK","PC 10/3 \"6\""]
["TECHNIK","PC 10/3 \"7\""]
["TECHNIK","PC 10/3 \"8\""]
["TECHNIK","PC 10/3 \"9\""]
["TECHNIK","PC 10/3 \"A\""]
["TECHNIK","PC 10/3 \"L\""]
["TECHNIK","PC 10/3 \"X\""]
["TECHNIK","PC 20/12"]
["TECHNIK","PC 20/21"]
["TECHNIK","PC 20/3"]
["TECHNIK","PC 20/3 \"0\""]
["TECHNIK","PC 20/3 \"1\""]
["TECHNIK","PC 20/3 \"2\""]
["TECHNIK","PC 20/3 \"3\""]
["TECHNIK","PC 20/3 \"4\""]
["TECHNIK","PC 20/3 \"5\""]
["TECHNIK","PC 20/3 \"6\""]
["TECHNIK","PC 20/3 \"7\""]
["TECHNIK","PC 20/3 \"8\""]
["TECHNIK","PC 20/3 \"9\""]
["TECHNIK","PC 20/6 \"L1\""]
["TECHNIK","PC 20/6 \"L2\""]
["TECHNIK","PC 20/6 \"L3\""]
["TECHNIK","PC 30/12"]
["TECHNIK","PC 30/3"]
["TECHNIK","PC 30/3 \"0\""]
["TECHNIK","PC 30/3 \"1\""]
["TECHNIK","PC 30/3 \"2\""]
["TECHNIK","PC 30/3 \"3\""]
["TECHNIK","PC 30/3 \"4\""]
["TECHNIK","PC 30/3 \"5\""]
["TECHNIK","PC 30/3 \"6\""]
["TECHNIK","PC 30/3 \"7\""]
["TECHNIK","PC 30/3 \"8\""]
["TECHNIK","PC 30/3 \"9\""]
["TECHNIK","PC 30/6"]
["TECHNIK","PC 40/12."]
["TECHNIK","PC 40/15"]
["TECHNIK","PC 40/21"]
["TECHNIK","PC 40/4"]
["TECHNIK","PC 40/4 \"0\""]
["TECHNIK","PC 40/4 \"1\""]
["TECHNIK","PC 40/4 \"2\""]
["TECHNIK","PC 40/4 \"3\""]
["TECHNIK","PC 40/4 \"4\""]
["TECHNIK","PC 40/4 \"5\""]
["TECHNIK","PC 40/4 \"6\""]
["TECHNIK","PC 40/4 \"7\""]
["TECHNIK","PC 40/4 \"8\""]
["TECHNIK","PC 40/4 \"9\""]
["TECHNIK","PC 40/4 \"A\""]
["TECHNIK","PC 40/4 \"B\""]
["TECHNIK","PD 1"]
["TECHNIK","PD 4"]
["TECHNIK","PD 4N"]
["TECHNIK","PD 5"]
["TECHNIK","PD 5N"]
["TECHNIK","PDD 0525/1"]
["TECHNIK","PDD 0525/2"]
["TECHNIK","PDD 0525/3"]
["TECHNIK","PDI 0,5- 8 oranžová"]
["TECHNIK","PDI 0,75- 8 bílá"]
["TECHNIK","PDI 0,75-10 bílá"]
["TECHNIK","PDI 0525/1"]
["TECHNIK","PDI 0525/2"]
["TECHNIK","PDI 0525/3"]
["TECHNIK","PDI 1- 8 žlutá"]
["TECHNIK","PDI 1,5- 8 rudá"]
["TECHNIK","PDI 1,5-10 rudá"]
["TECHNIK","PDI 1-10 žlutá"]
["TECHNIK","PDI 1-6/1"]
["TECHNIK","PDI 1-6/2"]
["TECHNIK","PDI 1-6/3"]
["TECHNIK","PDI 2,5- 8 modrá"]
["TECHNIK","PDI 4-10 šedá"]
["TECHNIK","PDI 416/1"]
["TECHNIK","PDI 416/2"]
["TECHNIK","PDI 416/3"]
["TECHNIK","PDI 6-12 černá"]
["TECHNIK","PDN 0525/6"]
["TECHNIK","PDN 0525/8"]
["TECHNIK","PDN 416"]
["REIKU-B","PEDST-10F"]
["REIKU-B","PEDST-12F"]
["REIKU-B","PEDST-17F"]
["REIKU-B","PEDST-17G"]
["REIKU-B","PEDST-23F"]
["REIKU-B","PEDST-23G"]
["REIKU-B","PEDST-29F"]
["REIKU-B","PEDST-29G"]
["REIKU-B","PEDST-36G/F"]
["REIKU-B","PEDST-48G/F"]
["TECHNIK","PE-HB-05 černá"]
["TECHNIK","PE-HB-10 černá"]
["TECHNIK","PE-HB-15 černá"]
["TECHNIK","PE-HB-20 černá"]
["TECHNIK","PE-HB-50 černá"]
["TECHNIK","Pěna k ochraně rukou"]
["REIKU-G","PEREG-10F"]
["REIKU-G","PEREG-12F"]
["REIKU-G","PEREG-17F"]
["REIKU-G","PEREG-23F"]
["REIKU-G","PEREG-29F"]
["REIKU-G","PEREG-36M"]
["REIKU-G","PEREG-48M"]
["TECHNIK","PF 10/15"]
["TECHNIK","PF 10/21"]
["TECHNIK","PF 20/18"]
["TECHNIK","PFC04221KA4"]
["TECHNIK","PFC45080KA9"]
["TECHNIK","PK 2/4.40"]
["TECHNIK","PK 2/4.40 \"-\""]
["TECHNIK","PK 2/4.40 \"/\""]
["TECHNIK","PK 2/4.40 \"0\""]
["TECHNIK","PK 2/4.40 \"1\""]
["TECHNIK","PK 2/4.40 \"2\""]
["TECHNIK","PK 2/4.40 \"3\""]
["TECHNIK","PK 2/4.40 \"4\""]
["TECHNIK","PK 2/4.40 \"5\""]
["TECHNIK","PK 2/4.40 \"6\""]
["TECHNIK","PK 2/4.40 \"7\""]
["TECHNIK","PK 2/4.40 \"8\""]
["TECHNIK","PK 2/4.40 \"9\""]
["TECHNIK","PK 2/4.40 \"A\""]
["TECHNIK","PK 2/4.40 \"B\""]
["TECHNIK","PK 2/4.40 \"C\""]
["TECHNIK","PK 2/4.40 \"D\""]
["TECHNIK","PK 2/4.40 \"E\""]
["TECHNIK","PK 2/4.40 \"F\""]
["TECHNIK","PK 2/4.40 \"G\""]
["TECHNIK","PK 2/4.40 \"H\""]
["TECHNIK","PK 2/4.40 \"I\""]
["TECHNIK","PK 2/4.40 \"J\""]
["TECHNIK","PK 2/4.40 \"K\""]
["TECHNIK","PK 2/4.40 \"L\""]
["TECHNIK","PK 2/4.40 \"M\""]
["TECHNIK","PK 2/4.40 \"N\""]
["TECHNIK","PK 2/4.40 \"O\""]
["TECHNIK","PK 2/4.40 \"P\""]
["TECHNIK","PK 2/4.40 \"Q\""]
["TECHNIK","PK 2/4.40 \"R\""]
["TECHNIK","PK 2/4.40 \"S\""]
["TECHNIK","PK 2/4.40 \"T\""]
["TECHNIK","PK 2/4.40 \"U\""]
["TECHNIK","PK 2/4.40 \"V\""]
["TECHNIK","PK 2/4.40 \"W\""]
["TECHNIK","PK 2/4.40 \"X\""]
["TECHNIK","PK 2/4.40 \"Y\""]
["TECHNIK","PK 2/4.40 \"Z\""]
["TECHNIK","PK 2/5 \"0\""]
["TECHNIK","PK 2/5 \"1\""]
["TECHNIK","PK 2/5 \"2\""]
["TECHNIK","PK 2/5 \"3\""]
["TECHNIK","PK 2/5 \"4\""]
["TECHNIK","PK 2/5 \"5\""]
["TECHNIK","PK 2/5 \"6\""]
["TECHNIK","PK 2/5 \"7\""]
["TECHNIK","PK 2/5 \"8\""]
["TECHNIK","PK 2/5 \"9\""]
["TECHNIK","PKH 65"]
["TECHNIK","PKH 70"]
["TECHNIK","PKH 70 POL"]
["TECHNIK","PKH100"]
["TECHNIK","PKH110 POL"]
["REIKU-B","PKNOB-07M081"]
["REIKU-B","PKNOB-07M121"]
["REIKU-G","PKNOG-07M081"]
["REIKU-G","PKNOG-07M121"]
["TECHNIK","PKR 68 B"]
["TECHNIK","PKRC 28 B"]
["TECHNIK","PKRC 48 B"]
["TECHNIK","PKRC 68 A"]
["TECHNIK","PKRC 68 B"]
["TECHNIK","PKRC 68 C"]
["TECHNIK","PKRC 68 D"]
["TECHNIK","PKRC 68 E"]
["TECHNIK","PKZ 2/6"]
["TECHNIK","PKZ 2/6 \"-\""]
["TECHNIK","PKZ 2/6 \".\""]
["TECHNIK","PKZ 2/6 \"0\""]
["TECHNIK","PKZ 2/6 \"1\""]
["TECHNIK","PKZ 2/6 \"2\""]
["TECHNIK","PKZ 2/6 \"3\""]
["TECHNIK","PKZ 2/6 \"4\""]
["TECHNIK","PKZ 2/6 \"5\""]
["TECHNIK","PKZ 2/6 \"6\""]
["TECHNIK","PKZ 2/6 \"7\""]
["TECHNIK","PKZ 2/6 \"8\""]
["TECHNIK","PKZ 2/6 \"9\""]
["TECHNIK","PKZ 2/6 \"A\""]
["TECHNIK","PKZ 2/6 \"B\""]
["TECHNIK","PKZ 2/6 \"C\""]
["TECHNIK","PKZ 2/6 \"D\""]
["TECHNIK","PKZ 2/6 \"E\""]
["TECHNIK","PKZ 2/6 \"F\""]
["TECHNIK","PKZ 2/6 \"G\""]
["TECHNIK","PKZ 2/6 \"H\""]
["TECHNIK","PKZ 2/6 \"K\""]
["TECHNIK","PKZ 2/6 \"L\""]
["TECHNIK","PKZ 2/6 \"M\""]
["TECHNIK","PKZ 2/6 \"N\""]
["TECHNIK","PKZ 2/6 \"O\""]
["TECHNIK","PKZ 2/6 \"P\""]
["TECHNIK","PKZ 2/6 \"R\""]
["TECHNIK","PKZ 2/6 \"S\""]
["TECHNIK","PKZ 2/6 \"T\""]
["TECHNIK","PKZ 2/6 \"U\""]
["TECHNIK","PKZ 2/6 \"V\""]
["TECHNIK","PKZ 2/6 \"W\""]
["TECHNIK","PKZ 2/6 \"X\""]
["TECHNIK","PKZ 2/6 \"Y\""]
["TECHNIK","PKZ 2/6 \"Z\""]
["TECHNIK","PL 150"]
["TECHNIK","PL 150 K"]
["TECHNIK","PL 200"]
["TECHNIK","PL 200 baterie"]
["TECHNIK","PL 200 K"]
["TECHNIK","PL 200 kufřík"]
["TECHNIK","PL 300"]
["TECHNIK","PL 300 baterie"]
["TECHNIK","PL 300 K"]
["TECHNIK","PLD \"0\""]
["TECHNIK","PLD \"0-9\""]
["TECHNIK","PLD \"1\""]
["TECHNIK","PLD \"2\""]
["TECHNIK","PLD \"3\""]
["TECHNIK","PLD \"4\""]
["TECHNIK","PLD \"5\""]
["TECHNIK","PLD \"6\""]
["TECHNIK","PLD \"7\""]
["TECHNIK","PLD \"8\""]
["TECHNIK","PLD \"9\""]
["TECHNIK","PLD \"L\""]
["TECHNIK","PLD \"L1\""]
["TECHNIK","PLD \"S\""]
["TECHNIK","PLD \"zem\""]
["TECHNIK","PLD color"]
["TECHNIK","PLD elektro"]
["TECHNIK","PLD komplet"]
["TECHNIK","PLD pouzdro"]
["TECHNIK","PM 10/33"]
["TECHNIK","PM 20/33"]
["TECHNIK","PM 20/45"]
["TECHNIK","PM 20/66"]
["TECHNIK","PM 24/33"]
["TECHNIK","PM 24/66"]
["REIKU-B","PMAOB-07P07"]
["REIKU-B","PMAOB-10P09"]
["REIKU-B","PMAOB-12P11"]
["REIKU-B","PMAOB-17P16"]
["REIKU-B","PMAOB-23P21"]
["REIKU-B","PMAOB-29P29"]
["REIKU-G","PMAOG-07P07"]
["REIKU-G","PMAOG-10P09"]
["REIKU-G","PMAOG-12P11"]
["REIKU-G","PMAOG-17P16"]
["REIKU-G","PMAOG-23P21"]
["REIKU-G","PMAOG-29P29"]
["REIKU-B","PMAVB-07P07"]
["REIKU-B","PMAVB-10P09"]
["REIKU-B","PMAVB-12P11"]
["REIKU-B","PMAVB-17P16"]
["REIKU-B","PMAVB-23P21"]
["REIKU-B","PMAVB-29P29"]
["REIKU-G","PMAVG-07P07"]
["REIKU-G","PMAVG-10P09"]
["REIKU-G","PMAVG-12P11"]
["REIKU-G","PMAVG-17P16"]
["REIKU-G","PMAVG-23P21"]
["REIKU-G","PMAVG-29P29"]
["REIKU-B","PMGMB-M20"]
["REIKU-B","PMGMB-M25"]
["REIKU-B","PMGMB-M32"]
["REIKU-B","PMGMB-M40"]
["REIKU-B","PMGOB-07M12Z"]
["REIKU-B","PMGOB-07P07"]
["REIKU-B","PMGOB-07P07Z"]
["REIKU-B","PMGOB-10M16"]
["REIKU-B","PMGOB-10M16Z"]
["REIKU-B","PMGOB-10M20"]
["REIKU-B","PMGOB-10P09"]
["REIKU-B","PMGOB-10P09Z"]
["REIKU-B","PMGOB-12M16"]
["REIKU-B","PMGOB-12M16Z"]
["REIKU-B","PMGOB-12M20"]
["REIKU-B","PMGOB-12M20Z"]
["REIKU-B","PMGOB-12P11"]
["REIKU-B","PMGOB-12P11Z"]
["REIKU-B","PMGOB-12P13Z"]
["REIKU-B","PMGOB-17M20"]
["REIKU-B","PMGOB-17M20Z"]
["REIKU-B","PMGOB-17M25"]
["REIKU-B","PMGOB-17P13"]
["REIKU-B","PMGOB-17P16"]
["REIKU-B","PMGOB-17P16Z"]
["REIKU-B","PMGOB-23M25"]
["REIKU-B","PMGOB-23M25Z"]
["REIKU-B","PMGOB-23M32"]
["REIKU-B","PMGOB-23P21"]
["REIKU-B","PMGOB-23P21Z"]
["REIKU-B","PMGOB-29M32"]
["REIKU-B","PMGOB-29M32Z"]
["REIKU-B","PMGOB-29M40"]
["REIKU-B","PMGOB-29P29"]
["REIKU-B","PMGOB-29P29Z"]
["REIKU-B","PMGOB-36M40Z"]
["REIKU-B","PMGOB-36M50"]
["REIKU-B","PMGOB-36P36"]
["REIKU-B","PMGOB-36P36Z"]
["REIKU-B","PMGOB-48M63"]
["REIKU-B","PMGOB-48M63Z"]
["REIKU-B","PMGOB-48P48"]
["REIKU-B","PMGOB-48P48Z"]
["REIKU-G","PMGOG-07M12Z"]
["REIKU-G","PMGOG-07P07"]
["REIKU-G","PMGOG-07P07Z"]
["REIKU-G","PMGOG-10M16"]
["REIKU-G","PMGOG-10M16Z"]
["REIKU-G","PMGOG-10M20"]
["REIKU-G","PMGOG-10P09"]
["REIKU-G","PMGOG-10P09Z"]
["REIKU-G","PMGOG-12M16"]
["REIKU-G","PMGOG-12M16Z"]
["REIKU-G","PMGOG-12M20"]
["REIKU-G","PMGOG-12M20Z"]
["REIKU-G","PMGOG-12P11"]
["REIKU-G","PMGOG-12P11Z"]
["REIKU-G","PMGOG-12P13Z"]
["REIKU-G","PMGOG-17M20"]
["REIKU-G","PMGOG-17M20Z"]
["REIKU-G","PMGOG-17M25"]
["REIKU-G","PMGOG-17P13"]
["REIKU-G","PMGOG-17P16"]
["REIKU-G","PMGOG-17P16Z"]
["REIKU-G","PMGOG-23M25"]
["REIKU-G","PMGOG-23M25Z"]
["REIKU-G","PMGOG-23M32"]
["REIKU-G","PMGOG-23P21"]
["REIKU-G","PMGOG-23P21Z"]
["REIKU-G","PMGOG-29M32"]
["REIKU-G","PMGOG-29M32Z"]
["REIKU-G","PMGOG-29M40"]
["REIKU-G","PMGOG-29P29"]
["REIKU-G","PMGOG-29P29Z"]
["REIKU-G","PMGOG-36M40Z"]
["REIKU-G","PMGOG-36M50"]
["REIKU-G","PMGOG-36P36"]
["REIKU-G","PMGOG-36P36Z"]
["REIKU-G","PMGOG-48M63"]
["REIKU-G","PMGOG-48M63Z"]
["REIKU-G","PMGOG-48P48"]
["REIKU-G","PMGOG-48P48Z"]
["REIKU-B","PMGVB-07M12Z"]
["REIKU-B","PMGVB-07P07"]
["REIKU-B","PMGVB-07P07Z"]
["REIKU-B","PMGVB-10M16"]
["REIKU-B","PMGVB-10M16Z"]
["REIKU-B","PMGVB-10M20"]
["REIKU-B","PMGVB-10P09"]
["REIKU-B","PMGVB-10P09Z"]
["REIKU-B","PMGVB-12M16"]
["REIKU-B","PMGVB-12M16Z"]
["REIKU-B","PMGVB-12M20"]
["REIKU-B","PMGVB-12M20Z"]
["REIKU-B","PMGVB-12P11"]
["REIKU-B","PMGVB-12P11Z"]
["REIKU-B","PMGVB-12P13Z"]
["REIKU-B","PMGVB-17M20"]
["REIKU-B","PMGVB-17M20Z"]
["REIKU-B","PMGVB-17M25"]
["REIKU-B","PMGVB-17P13"]
["REIKU-B","PMGVB-17P16"]
["REIKU-B","PMGVB-17P16Z"]
["REIKU-B","PMGVB-23M25"]
["REIKU-B","PMGVB-23M25Z"]
["REIKU-B","PMGVB-23M32"]
["REIKU-B","PMGVB-23P21"]
["REIKU-B","PMGVB-23P21Z"]
["REIKU-B","PMGVB-29M32"]
["REIKU-B","PMGVB-29M32Z"]
["REIKU-B","PMGVB-29M40"]
["REIKU-B","PMGVB-29P29"]
["REIKU-B","PMGVB-29P29Z"]
["REIKU-B","PMGVB-36M40Z"]
["REIKU-B","PMGVB-36M50"]
["REIKU-B","PMGVB-36P36"]
["REIKU-B","PMGVB-36P36Z"]
["REIKU-B","PMGVB-48M63"]
["REIKU-B","PMGVB-48M63Z"]
["REIKU-B","PMGVB-48P48"]
["REIKU-B","PMGVB-48P48Z"]
["REIKU-G","PMGVG-07M12Z"]
["REIKU-G","PMGVG-07P07"]
["REIKU-G","PMGVG-07P07Z"]
["REIKU-G","PMGVG-10M16"]
["REIKU-G","PMGVG-10M16Z"]
["REIKU-G","PMGVG-10M20"]
["REIKU-G","PMGVG-10P09"]
["REIKU-G","PMGVG-10P09Z"]
["REIKU-G","PMGVG-12M16"]
["REIKU-G","PMGVG-12M16Z"]
["REIKU-G","PMGVG-12M20"]
["REIKU-G","PMGVG-12M20Z"]
["REIKU-G","PMGVG-12P11"]
["REIKU-G","PMGVG-12P11Z"]
["REIKU-G","PMGVG-12P13Z"]
["REIKU-G","PMGVG-17M20"]
["REIKU-G","PMGVG-17M20Z"]
["REIKU-G","PMGVG-17M25"]
["REIKU-G","PMGVG-17P13"]
["REIKU-G","PMGVG-17P16"]
["REIKU-G","PMGVG-17P16Z"]
["REIKU-G","PMGVG-23M25"]
["REIKU-G","PMGVG-23M25Z"]
["REIKU-G","PMGVG-23M32"]
["REIKU-G","PMGVG-23P21"]
["REIKU-G","PMGVG-23P21Z"]
["REIKU-G","PMGVG-29M32"]
["REIKU-G","PMGVG-29M32Z"]
["REIKU-G","PMGVG-29M40"]
["REIKU-G","PMGVG-29P29"]
["REIKU-G","PMGVG-29P29Z"]
["REIKU-G","PMGVG-36M40Z"]
["REIKU-G","PMGVG-36M50"]
["REIKU-G","PMGVG-36P36"]
["REIKU-G","PMGVG-36P36Z"]
["REIKU-G","PMGVG-48M63"]
["REIKU-G","PMGVG-48M63Z"]
["REIKU-G","PMGVG-48P48"]
["REIKU-G","PMGVG-48P48Z"]
["REIKU-B","PMSOB-07P07"]
["REIKU-G","PMSOG-07P07"]
["REIKU-B","PMSVB-07P07"]
["REIKU-G","PMSVG-07P07"]
["REIKU-B","PMWOB-10P09"]
["REIKU-B","PMWOB-12M16"]
["REIKU-B","PMWOB-12P11"]
["REIKU-B","PMWOB-17M20"]
["REIKU-B","PMWOB-17P13"]
["REIKU-B","PMWOB-17P16"]
["REIKU-B","PMWOB-23M25"]
["REIKU-B","PMWOB-23P21"]
["REIKU-B","PMWOB-29M32"]
["REIKU-B","PMWOB-29P29"]
["REIKU-B","PMWOB-36M40"]
["REIKU-B","PMWOB-36P36"]
["REIKU-B","PMWOB-48M50"]
["REIKU-B","PMWOB-48P48"]
["REIKU-G","PMWOG-10P09"]
["REIKU-G","PMWOG-12M16"]
["REIKU-G","PMWOG-12P11"]
["REIKU-G","PMWOG-17M20"]
["REIKU-G","PMWOG-17P13"]
["REIKU-G","PMWOG-17P16"]
["REIKU-G","PMWOG-23M25"]
["REIKU-G","PMWOG-23P21"]
["REIKU-G","PMWOG-29M32"]
["REIKU-G","PMWOG-29P29"]
["REIKU-G","PMWOG-36M40"]
["REIKU-G","PMWOG-36P36"]
["REIKU-G","PMWOG-48M50"]
["REIKU-G","PMWOG-48P48"]
["REIKU-B","PMWVB-10P09"]
["REIKU-B","PMWVB-12M16"]
["REIKU-B","PMWVB-12P11"]
["REIKU-B","PMWVB-17M20"]
["REIKU-B","PMWVB-17P13"]
["REIKU-B","PMWVB-17P16"]
["REIKU-B","PMWVB-23M25"]
["REIKU-B","PMWVB-23P21"]
["REIKU-B","PMWVB-29M32"]
["REIKU-B","PMWVB-29P29"]
["REIKU-B","PMWVB-36M40"]
["REIKU-B","PMWVB-36P36"]
["REIKU-B","PMWVB-48M50"]
["REIKU-B","PMWVB-48P48"]
["REIKU-G","PMWVG-10P09"]
["REIKU-G","PMWVG-12M16"]
["REIKU-G","PMWVG-12P11"]
["REIKU-G","PMWVG-17M20"]
["REIKU-G","PMWVG-17P13"]
["REIKU-G","PMWVG-17P16"]
["REIKU-G","PMWVG-23M25"]
["REIKU-G","PMWVG-23P21"]
["REIKU-G","PMWVG-29M32"]
["REIKU-G","PMWVG-29P29"]
["REIKU-G","PMWVG-36M40"]
["REIKU-G","PMWVG-36P36"]
["REIKU-G","PMWVG-48M50"]
["REIKU-G","PMWVG-48P48"]
["TECHNIK","PN  1"]
["TECHNIK","PN  8"]
["TECHNIK","PN  8/1"]
["TECHNIK","PN 12"]
["TECHNIK","PN 14K"]
["TECHNIK","PN 16"]
["TECHNIK","PN 16/1"]
["TECHNIK","PN 16/1 STRIP"]
["TECHNIK","PN 16/1000"]
["TECHNIK","PN 16/1P"]
["TECHNIK","PN 16/P"]
["TECHNIK","PN 24"]
["TECHNIK","PN 25"]
["TECHNIK","PN 25/1"]
["TECHNIK","PN 25/1000"]
["TECHNIK","PN 26T"]
["TECHNIK","PN 26TL"]
["TECHNIK","PN 27"]
["TECHNIK","PN 27/1000"]
["TECHNIK","PN 30"]
["TECHNIK","PN 30K"]
["TECHNIK","PN 48"]
["TECHNIK","PN 50"]
["TECHNIK","PN 50K"]
["TECHNIK","PN 56P"]
["TECHNIK","PN DATA"]
["TECHNIK","PN OPTI"]
["TECHNIK","PNFE  3/5"]
["TECHNIK","PNFE  4-6"]
["TECHNIK","PNFE  4-6 P"]
["TECHNIK","PNFE  5/7"]
["TECHNIK","PNFE  7/10"]
["TECHNIK","PNFE  9/12"]
["TECHNIK","PNFE 11/16"]
["TECHNIK","PNFE 40x4"]
["TECHNIK","PNFE B  4/6"]
["TECHNIK","PNFE B  7/10"]
["TECHNIK","PNFE B 10/14"]
["TECHNIK","PNFE U  5-8"]
["TECHNIK","PNFE U  7-9"]
["TECHNIK","PNFE U  8-11"]
["TECHNIK","PNFE U  9-13"]
["TECHNIK","PNFE. 4-5"]
["TECHNIK","PNFE. 5-7"]
["TECHNIK","PNFE. 6-8"]
["TECHNIK","PNFE. 8-10"]
["TECHNIK","PNFE.10-13"]
["TECHNIK","PNFE.11-16"]
["TECHNIK","PNFE.13-18"]
["TECHNIK SPECIAL - AKCIA","PO 7000"]
["TECHNIK","PO-04000BN4"]
["TECHNIK","PO-04000DN4"]
["TECHNIK","PO-04000SN4"]
["TECHNIK","PO-05000BN4"]
["TECHNIK","PO-05000DN4"]
["TECHNIK","PO-05000SN4"]
["TECHNIK","PO-06000BN4"]
["TECHNIK","PO-06000BN9"]
["TECHNIK","PO-06000DN4"]
["TECHNIK","PO-06000SN4"]
["TECHNIK","PO-068TWBN4"]
["TECHNIK","PO-06Q10KN4"]
["TECHNIK","PO-07000DN4"]
["TECHNIK","PO-07000SN4"]
["TECHNIK","PO-08000BN4"]
["TECHNIK SPECIAL - AKCIA","PODLOŽKY 3"]
["TECHNIK SPECIAL - AKCIA","PODLOŽKY 5"]
["REIKU-B","POFHB-23/29"]
["REIKU-B","POFHB-36"]
["REIKU-B","POFHB-36/36"]
["REIKU-B","POGTB-70"]
["TECHNIK","POH07060AA0"]
["TECHNIK","POH12082AA0"]
["REIKU-B","POKGB-70"]
["REIKU-B","POSSB-90K"]
["REIKU-B","POSSB-90M"]
["TECHNIK","Pouzdro E"]
["TECHNIK","Pouzdro V"]
["TECHNIK","POZ02000KN4"]
["TECHNIK","POZ10000SN4"]
["TECHNIK SPECIAL - AKCIA","PP 600 adaptér"]
["TECHNIK SPECIAL - AKCIA","PP 600 držák"]
["TECHNIK SPECIAL - AKCIA","PP 600 pedál"]
["TECHNIK SPECIAL - AKCIA","PP 600 tubus"]
["TECHNIK SPECIAL - AKCIA","PP 600-D 01410"]
["TECHNIK SPECIAL - AKCIA","PP 600-D 1025"]
["TECHNIK SPECIAL - AKCIA","PP 600-MO 011"]
["TECHNIK SPECIAL - AKCIA","PP 600-MO 0525"]
["TECHNIK SPECIAL - AKCIA","PP 600-MO 056"]
["TECHNIK SPECIAL - AKCIA","PP 600-OI 056"]
["TECHNIK SPECIAL - AKCIA","PP 600-OL 410"]
["TECHNIK SPECIAL - AKCIA","PP 600-ON 0110"]
["TECHNIK SPECIAL - AKCIA","PP 80"]
["TECHNIK SPECIAL - AKCIA","PP 80K"]
["TECHNIK","PP NIT  50"]
["TECHNIK","PP NIT  75"]
["TECHNIK","PP NIT 125"]
["TECHNIK","PP NIT 175"]
["TECHNIK","PP NIT 225"]
["TECHNIK","PP+04600SN4"]
["TECHNIK","PPA09000SN4"]
["TECHNIK","PPB  6"]
["TECHNIK","PPB  8"]
["TECHNIK","PPB 10"]
["TECHNIK","PPB 15"]
["REIKU-B","PPREB-12F"]
["REIKU-B","PPREB-17F"]
["REIKU-B","PPREB-23'F"]
["REIKU-B","PPREB-29F"]
["REIKU-B","PPREB-36F"]
["REIKU-B","PPREB-48F"]
["REIKU-B","PPRTB-10"]
["REIKU-B","PPRTB-12"]
["REIKU-B","PPRTB-14"]
["REIKU-B","PPRTB-17"]
["REIKU-B","PPRTB-24"]
["REIKU-B","PPRTB-29"]
["REIKU-B","PPRTB-34"]
["REIKU-B","PPRTB-45"]
["REIKU-B","PPRTB-68"]
["TECHNIK SPECIAL - AKCIA","PPV 120/12"]
["TECHNIK SPECIAL - AKCIA","PPV 120/12 DD"]
["TECHNIK SPECIAL - AKCIA","PPV 120/12 DMS"]
["TECHNIK SPECIAL - AKCIA","PPV 120/12 MMS"]
["TECHNIK SPECIAL - AKCIA","PPV 120/12 OM"]
["TECHNIK SPECIAL - AKCIA","PPV 160/10"]
["TECHNIK","PR 7/16"]
["TECHNIK","PRI 68/ 2"]
["TECHNIK","PRI 68/ 3"]
["TECHNIK","PRI 68/ 4"]
["TECHNIK","PRI 68/24"]
["TECHNIK","PRIK 28/ 2"]
["TECHNIK","PRIK 28/ 3"]
["TECHNIK","PRIK 28/ 4"]
["TECHNIK","PRIK 28/ 6"]
["TECHNIK","PRIK 28/24"]
["TECHNIK","PRIK 28/36"]
["TECHNIK","PRIK 48/ 2"]
["TECHNIK","PRIK 48/ 4"]
["TECHNIK","PRIK 48/24"]
["TECHNIK","PRIK 68/ 2"]
["TECHNIK","PRIK 68/ 4"]
["TECHNIK","PRIK 68/24"]
["TECHNIK","PROFIPOL"]
["TECHNIK","PS 135"]
["TECHNIK","PSK 18000"]
["TECHNIK","PSK 18001"]
["TECHNIK","PSK 18002"]
["REIKU-B","PSNOB-07M081"]
["REIKU-B","PSNOB-07M121"]
["REIKU-G","PSNOG-07M081"]
["REIKU-G","PSNOG-07M121"]
["TECHNIK","PT 02/15"]
["TECHNIK","PT 02/21"]
["TECHNIK","PT 10/15"]
["TECHNIK","PT 10/21"]
["TECHNIK SPECIAL - AKCIA","PT 10-22"]
["TECHNIK SPECIAL - AKCIA","PT 16-22"]
["TECHNIK","PT 20/15"]
["TECHNIK","PT 20/21"]
["TECHNIK SPECIAL - AKCIA","PT 25-22"]
["TECHNIK","PT 30/15"]
["TECHNIK","PT 30/21"]
["TECHNIK","PT 30/30"]
["TECHNIK SPECIAL - AKCIA","PT 35-22"]
["TECHNIK","PT 40/15"]
["TECHNIK","PT 40/21"]
["TECHNIK","PT 40/30"]
["TECHNIK SPECIAL - AKCIA","PT 50-22"]
["TECHNIK SPECIAL - AKCIA","PT 70-22"]
["TECHNIK SPECIAL - AKCIA","PT 70-C"]
["TECHNIK SPECIAL - AKCIA","PT 95-22"]
["TECHNIK SPECIAL - AKCIA","PT 95-C"]
["TECHNIK SPECIAL - AKCIA","PT120-22"]
["TECHNIK SPECIAL - AKCIA","PT120-C"]
["TECHNIK SPECIAL - AKCIA","PT150-22"]
["TECHNIK SPECIAL - AKCIA","PT150-C"]
["TECHNIK SPECIAL - AKCIA","PT185-22"]
["TECHNIK SPECIAL - AKCIA","PT185-C"]
["TECHNIK SPECIAL - AKCIA","PT240-22"]
["TECHNIK SPECIAL - AKCIA","PT240-C"]
["TECHNIK","PT-3600"]
["TECHNIK","PT-9600 + kufr"]
["TECHNIK","PT-9700 PC"]
["TECHNIK","PT-9800PCN"]
["TECHNIK","PTC 10/15"]
["TECHNIK","PTC 10/21"]
["TECHNIK","PTC 10/30"]
["TECHNIK","PTC 20/15"]
["TECHNIK","PTC 20/21"]
["TECHNIK","PTC 20/30"]
["TECHNIK","PTC 30/15"]
["TECHNIK","PTC 30/21"]
["TECHNIK","PTC 30/30"]
["TECHNIK","PTC 40/15"]
["TECHNIK","PTC 40/21"]
["TECHNIK","PTC 40/30"]
["TECHNIK","PTC 50/15"]
["TECHNIK","PTC 50/21"]
["TECHNIK","PTC 50/30"]
["TECHNIK","PT-D200 BW"]
["TECHNIK","PT-D200 BW VP"]
["TECHNIK","PT-D200 VP"]
["TECHNIK","PT-D450 VP"]
["TECHNIK","PT-D600 VP"]
["TECHNIK","PT-E100 VP+kufr"]
["TECHNIK","PT-E300 VP+kufr"]
["TECHNIK","PT-E550WVP+kufr AKCE"]
["TECHNIK","PT-H105 WB"]
["TECHNIK","PT-H300"]
["TECHNIK","PT-H500"]
["TECHNIK","PTM 20"]
["TECHNIK","PTM 30"]
["TECHNIK","PTM 40"]
["TECHNIK","PT-P700"]
["TECHNIK","PT-P750 W"]
["TECHNIK","PTS 48"]
["REIKU-B","PURMB-70G"]
["REIKU-B","PURRB-07G"]
["REIKU-B","PURRB-10F"]
["REIKU-B","PURRB-12F"]
["REIKU-B","PURRB-17F"]
["REIKU-B","PURRB-17G"]
["REIKU-B","PURRB-23F"]
["REIKU-B","PURRB-23G"]
["REIKU-B","PURRB-29F"]
["REIKU-B","PURRB-29G"]
["REIKU-B","PURRB-36F"]
["REIKU-B","PURRB-36G"]
["REIKU-B","PURRB-42M"]
["REIKU-B","PURRB-48F"]
["REIKU-B","PURRB-48G"]
["REIKU-B","PURRB-52G"]
["REIKU-B","PURRB-68G"]
["REIKU-B","PURRB-70G"]
["REIKU-B","PURRB-95G"]
["REIKU-B","PURVB-36G"]
["REIKU-B","PURVB-48F"]
["REIKU-B","PURVB-52G"]
["REIKU-B","PURVB-70G"]
["TECHNIK SPECIAL - AKCIA","PW 10-16 C"]
["TECHNIK SPECIAL - AKCIA","PW 25-35 C"]
["TECHNIK SPECIAL - AKCIA","PW 50-70 C"]
["TECHNIK SPECIAL - AKCIA","PW 95-150 C"]
["TECHNIK SPECIAL - AKCIA","PW185-240 C"]
["REIKU-B","PWNOB-07M081"]
["REIKU-B","PWNOB-07M121"]
["REIKU-B","PWNOB-07M181"]
["REIKU-B","PWNOB-07M301"]
["REIKU-G","PWNOG-07M081"]
["REIKU-G","PWNOG-07M121"]
["REIKU-G","PWNOG-07M181"]
["REIKU-G","PWNOG-07M301"]
["TECHNIK","PZ 1,5"]
["TECHNIK","PZ 10 HEX"]
["TECHNIK","PZ 10 SQR"]
["TECHNIK","QL 1050"]
["TECHNIK","QL 1060 N"]
["TECHNIK","QL 570"]
["TECHNIK","QL 650 TD"]
["TECHNIK","QL 700"]
["TECHNIK","QL 710 W"]
["TECHNIK","QL 720 NW"]
["TECHNIK SPECIAL - AKCIA","R+M ovál  9,5x20"]
["TECHNIK SPECIAL - AKCIA","R+M ovál 11,0x20"]
["TECHNIK SPECIAL - AKCIA","R+M ovál 12,5x20"]
["TECHNIK SPECIAL - AKCIA","R+M ovál 13,5x20"]
["TECHNIK SPECIAL - AKCIA","RAZNÍK  6,6"]
["TECHNIK SPECIAL - AKCIA","RAZNÍK  9,0"]
["TECHNIK SPECIAL - AKCIA","RAZNÍK  9,5"]
["TECHNIK SPECIAL - AKCIA","RAZNÍK 11,0"]
["TECHNIK SPECIAL - AKCIA","RAZNÍK 13,5"]
["TECHNIK SPECIAL - AKCIA","RAZNÍK 17,5"]
["TECHNIK SPECIAL - AKCIA","RAZNÍK 21,5"]
["TECHNIK","RBH  15/6"]
["TECHNIK","RBH  25/10"]
["TECHNIK","RBH  30/12"]
["TECHNIK","RBH  40/16"]
["TECHNIK","RBH  50/20"]
["TECHNIK","RBH  65/25"]
["TECHNIK","RBH  75/30"]
["TECHNIK","RBH  85/35"]
["TECHNIK","RBH 100/40"]
["TECHNIK","RBH 120/50"]
["TECHNIK","RBH 150/60"]
["TECHNIK SPECIAL - AKCIA","RC 300"]
["TECHNIK SPECIAL - AKCIA","RC 500"]
["TECHNIK SPECIAL - AKCIA","RC 500 L65"]
["TECHNIK SPECIAL - AKCIA","RC 500 R64"]
["TECHNIK SPECIAL - AKCIA","RC 500 R84"]
["TECHNIK","RCK  3/1 černá"]
["TECHNIK","RCK  3/1 modrá"]
["TECHNIK","RCK  3/1 rudá"]
["TECHNIK","RCK  3/1 transp"]
["TECHNIK","RCK  3/1 zelená"]
["TECHNIK","RCK  3/1 žlutá"]
["TECHNIK","RCK  4/1 černá"]
["TECHNIK","RCK  4/1 modrá"]
["TECHNIK","RCK  4/1 rudá"]
["TECHNIK","RCK  4/1 transp"]
["TECHNIK","RCK  4/1 zelená"]
["TECHNIK","RCK  4/1 žlutá"]
["TECHNIK","RCK  6/2 černá"]
["TECHNIK","RCK  6/2 hnědá"]
["TECHNIK","RCK  6/2 modrá"]
["TECHNIK","RCK  6/2 rudá"]
["TECHNIK","RCK  6/2 transp"]
["TECHNIK","RCK  6/2 zelená"]
["TECHNIK","RCK  6/2 žlutá"]
["TECHNIK","RCK  8/2 černá"]
["TECHNIK","RCK  8/2 černá R"]
["TECHNIK","RCK  8/2 hnědá"]
["TECHNIK","RCK  8/2 modrá"]
["TECHNIK","RCK  8/2 rudá"]
["TECHNIK","RCK  8/2 transp"]
["TECHNIK","RCK  8/2 zelená"]
["TECHNIK","RCK  8/2 žlutá"]
["TECHNIK","RCK 12/3 černá"]
["TECHNIK","RCK 12/3 modrá"]
["TECHNIK","RCK 12/3 rudá"]
["TECHNIK","RCK 12/3 transp"]
["TECHNIK","RCK 12/3 zelená"]
["TECHNIK","RCK 12/3 žlutá"]
["TECHNIK","RDK  76/18"]
["TECHNIK","RDK 105/32"]
["TECHNIK","RDK 140/34"]
["TECHNIK","RDK 155/90"]
["TECHNIK","RDK 175/77"]
["TECHNIK","RDK 185/42"]
["TECHNIK","RDK 225/90"]
["TECHNIK","RDK 245/125"]
["TECHNIK","RDK 350/125"]
["TECHNIK","RDK 390/200"]
["TECHNIK","RDK 500/200"]
["TECHNIK","RDK 710/250"]
["TECHNIK","RDK 820/315"]
["TECHNIK","RDK 920/315"]
["TECHNIK","RGK   9/3"]
["TECHNIK","RGK  12/4"]
["TECHNIK","RGK  19/3,2"]
["TECHNIK","RGK  22/6"]
["TECHNIK","RGK  33/5,5"]
["TECHNIK","RGK  33/8"]
["TECHNIK","RGK  44/7,4"]
["TECHNIK","RGK  45/13"]
["TECHNIK","RGK  51/8,3"]
["TECHNIK","RGK  55/16"]
["TECHNIK","RGK  65/19"]
["TECHNIK","RGK  69/11,7"]
["TECHNIK","RGK  75/22"]
["TECHNIK","RGK  85/25"]
["TECHNIK","RGK  89/17,1"]
["TECHNIK","RGK  95/30"]
["TECHNIK","RGK 105/30"]
["TECHNIK","RGK 115/34"]
["TECHNIK","RGK 119/22,9"]
["TECHNIK","RGK 130/36"]
["TECHNIK","RGK 140/34"]
["TECHNIK","RGK 160/50"]
["TECHNIK","RGK 175/50"]
["TECHNIK","RGK 200/60"]
["TECHNIK SPECIAL - AKCIA","RH 50"]
["TECHNIK SPECIAL - AKCIA","RHC 131"]
["TECHNIK SPECIAL - AKCIA","RHC 131 LN"]
["TECHNIK","RHINO 101-K"]
["TECHNIK","RHINO 101-O"]
["TECHNIK SPECIAL - AKCIA","RHM 132"]
["TECHNIK SPECIAL - AKCIA","RHT 160"]
["TECHNIK SPECIAL - AKCIA","RHT 160-60N"]
["TECHNIK SPECIAL - AKCIA","RHU 131-C"]
["TECHNIK SPECIAL - AKCIA","RHU 450"]
["TECHNIK SPECIAL - AKCIA","RHU 520"]
["TECHNIK SPECIAL - AKCIA","RHU1000"]
["TECHNIK","RJ 10"]
["TECHNIK","RJ 11"]
["TECHNIK","RJ 11-2F"]
["TECHNIK","RJ 11-2F/M"]
["TECHNIK","RJ 11-3F"]
["TECHNIK","RJ 12"]
["TECHNIK","RJ 45-2F"]
["TECHNIK","RJ 45-2F/M"]
["TECHNIK","RJ 45-3F"]
["TECHNIK","RJ 45-D"]
["TECHNIK","RJ 45-L"]
["TECHNIK","RJ 45-MDc6"]
["TECHNIK","RJ 45-MDc6v"]
["TECHNIK","RJ 45-MLc6"]
["TECHNIK","RJ 45-MLc6v"]
["TECHNIK","RJ 45-S2F"]
["TECHNIK","RJ 45-SCLIP"]
["TECHNIK","RJ 45-SD"]
["TECHNIK","RJ 45-SDc6"]
["TECHNIK","RJ 45-SDc6v"]
["TECHNIK","RJ 45-SL"]
["TECHNIK","RJ 45-SLc6"]
["TECHNIK","RJ 45-SLc6v"]
["TECHNIK","RJT CRONOtester"]
["TECHNIK","RJT LANtest"]
["TECHNIK","RJT TL-828A"]
["TECHNIK","RJT WS-SC8108"]
["TECHNIK","RM  22/6- 500"]
["TECHNIK","RM  22/6-1000"]
["TECHNIK","RM  42/8- 500"]
["TECHNIK","RM  42/8-1000"]
["TECHNIK","RM  42/8-1500"]
["TECHNIK","RM  62/22- 500"]
["TECHNIK","RM  62/22-1000"]
["TECHNIK","RM  62/22-1500"]
["TECHNIK","RM  92/30- 500"]
["TECHNIK","RM  92/30-1000"]
["TECHNIK","RM  92/30-1500"]
["TECHNIK","RM 122/38- 500"]
["TECHNIK","RM 122/38-1000"]
["TECHNIK","RM 122/38-1500"]
["TECHNIK","RM 160/40- 500"]
["TECHNIK","RM 160/40-1000"]
["TECHNIK","RM 210/55- 500"]
["TECHNIK","RM 210/55-1000"]
["TECHNIK","RM 210/55-1500"]
["TECHNIK","RN 25 F"]
["TECHNIK","RN 32"]
["TECHNIK","RN 32 KN"]
["TECHNIK","RN 32 KN/1000"]
["TECHNIK","RN 33"]
["TECHNIK","RN 34"]
["TECHNIK","RN 34 F"]
["TECHNIK","RN 34 M"]
["TECHNIK","RN 35 P"]
["TECHNIK","RN 38 T"]
["TECHNIK","RN 40 PB"]
["TECHNIK","RN 42 M"]
["TECHNIK","RN 45 P"]
["TECHNIK","RN 50 UNI SET"]
["TECHNIK","RN 52"]
["TECHNIK","RN 52 KN"]
["TECHNIK","RN 52 KN/1000"]
["TECHNIK","RN 52 M"]
["TECHNIK","RN 52 P"]
["TECHNIK","RN 52/1000"]
["TECHNIK","RN 53"]
["TECHNIK","RN 54"]
["TECHNIK","RN 55"]
["TECHNIK","RN 60"]
["TECHNIK","RN 60 KN"]
["TECHNIK","RN 60 KN/1000"]
["TECHNIK","RN 60T"]
["TECHNIK","RN 62 P"]
["TECHNIK","RN 62 S"]
["TECHNIK","RN 65"]
["TECHNIK","RN 80 S"]
["TECHNIK","RN 85 PB"]
["TECHNIK","RN 92"]
["TECHNIK","RN100"]
["TECHNIK","RN100T"]
["TECHNIK","RPK   8/2"]
["TECHNIK","RPK   9/3"]
["TECHNIK","RPK   9/3 žz"]
["TECHNIK","RPK  12/4"]
["TECHNIK","RPK  12/4 žz"]
["TECHNIK","RPK  16/5"]
["TECHNIK","RPK  17/3"]
["TECHNIK","RPK  19/6"]
["TECHNIK","RPK  22/6"]
["TECHNIK","RPK  22/6 žz"]
["TECHNIK","RPK  25/10 žz"]
["TECHNIK","RPK  25/8"]
["TECHNIK","RPK  28/9"]
["TECHNIK","RPK  33/11"]
["TECHNIK","RPK  33/8"]
["TECHNIK","RPK  35/12 žz"]
["TECHNIK","RPK  40/12"]
["TECHNIK","RPK  40/16 žz"]
["TECHNIK","RPK  55/16"]
["TECHNIK","RPK  65/19"]
["TECHNIK","RPK  75/22"]
["TECHNIK","RPK  85/25"]
["TECHNIK","RPK  95/25"]
["TECHNIK","RPK 115/34"]
["TECHNIK","RPK 140/42"]
["TECHNIK","RPK 160/50"]
["TECHNIK","RPK 175/58"]
["TECHNIK","RPK 210/65"]
["TECHNIK","RPK 230/75"]
["TECHNIK SPECIAL - AKCIA","RT  6,5"]
["TECHNIK SPECIAL - AKCIA","RT  7,0"]
["TECHNIK SPECIAL - AKCIA","RT  8,5"]
["TECHNIK SPECIAL - AKCIA","RT  9,0"]
["TECHNIK SPECIAL - AKCIA","RT 10,5"]
["TECHNIK SPECIAL - AKCIA","RT 11,0"]
["TECHNIK SPECIAL - AKCIA","RT 12,5"]
["TECHNIK SPECIAL - AKCIA","RT 13,0"]
["TECHNIK SPECIAL - AKCIA","RT 14,0"]
["TECHNIK SPECIAL - AKCIA","RT 14,5"]
["TECHNIK SPECIAL - AKCIA","RT 15,0"]
["TECHNIK SPECIAL - AKCIA","RT 17,0"]
["TECHNIK","RTE  4,8/2,8"]
["TECHNIK","RTE  6,1/3,5"]
["TECHNIK","RTE  7,7/4,4"]
["TECHNIK","RTE 10,9/6,9"]
["TECHNIK","RTE 11,9/8,5"]
["TECHNIK","RTE 12,7/3,2"]
["TECHNIK SPECIAL - AKCIA","RU  10-22"]
["TECHNIK SPECIAL - AKCIA","RU  10-50"]
["TECHNIK SPECIAL - AKCIA","RU  10-C"]
["TECHNIK SPECIAL - AKCIA","RU  16-22"]
["TECHNIK SPECIAL - AKCIA","RU  16-50"]
["TECHNIK SPECIAL - AKCIA","RU  16-C"]
["TECHNIK SPECIAL - AKCIA","RU  35/25-22"]
["TECHNIK SPECIAL - AKCIA","RU  35/25-50"]
["TECHNIK SPECIAL - AKCIA","RU  35/25-C"]
["TECHNIK SPECIAL - AKCIA","RU  50/35-22"]
["TECHNIK SPECIAL - AKCIA","RU  50/35-50"]
["TECHNIK SPECIAL - AKCIA","RU  50/35-C"]
["TECHNIK SPECIAL - AKCIA","RU  70/50-22"]
["TECHNIK SPECIAL - AKCIA","RU  70/50-50"]
["TECHNIK SPECIAL - AKCIA","RU  70/50-C"]
["TECHNIK SPECIAL - AKCIA","RU  95/70-22"]
["TECHNIK SPECIAL - AKCIA","RU  95/70-50"]
["TECHNIK SPECIAL - AKCIA","RU  95/70-C"]
["TECHNIK SPECIAL - AKCIA","RU 120/95-22"]
["TECHNIK SPECIAL - AKCIA","RU 120/95-3D"]
["TECHNIK SPECIAL - AKCIA","RU 120/95-50"]
["TECHNIK SPECIAL - AKCIA","RU 120/95-C"]
["TECHNIK SPECIAL - AKCIA","RU 150/120-22"]
["TECHNIK SPECIAL - AKCIA","RU 150/120-3D"]
["TECHNIK SPECIAL - AKCIA","RU 150/120-50"]
["TECHNIK SPECIAL - AKCIA","RU 150/120-C"]
["TECHNIK SPECIAL - AKCIA","RU 185/150-22"]
["TECHNIK SPECIAL - AKCIA","RU 185/150-3D"]
["TECHNIK SPECIAL - AKCIA","RU 185/150-50"]
["TECHNIK SPECIAL - AKCIA","RU 185/150-C"]
["TECHNIK SPECIAL - AKCIA","RU 240/185-22"]
["TECHNIK SPECIAL - AKCIA","RU 240/185-3D"]
["TECHNIK SPECIAL - AKCIA","RU 240/185-50"]
["TECHNIK SPECIAL - AKCIA","RU 240/185-C"]
["TECHNIK SPECIAL - AKCIA","RU 300/240-22"]
["TECHNIK SPECIAL - AKCIA","RU 300/240-3D"]
["TECHNIK SPECIAL - AKCIA","RU 300/240-50"]
["TECHNIK SPECIAL - AKCIA","RU 300/240-C"]
["TECHNIK SPECIAL - AKCIA","RU300-C"]
["TECHNIK","S"]
["TECHNIK SPECIAL - AKCIA","S 125"]
["TECHNIK","S 4-28 Voltage"]
["TECHNIK","S 4-28H"]
["TECHNIK","S0718040"]
["TECHNIK","S0718050"]
["TECHNIK","S0718060"]
["TECHNIK","S0718070"]
["TECHNIK","S0718080"]
["TECHNIK","S0718100"]
["TECHNIK","S0718120"]
["TECHNIK","S0718160"]
["TECHNIK","S0718170"]
["TECHNIK","S0718180"]
["TECHNIK","S0718200"]
["TECHNIK","S0718210"]
["TECHNIK","S0718220"]
["TECHNIK","S0718240"]
["TECHNIK","S0718260"]
["TECHNIK","S0718270"]
["TECHNIK","S0718280"]
["TECHNIK","S0718280.C"]
["TECHNIK","S0718290"]
["TECHNIK","S0718290.C"]
["TECHNIK","S0718300"]
["TECHNIK","S0718300.C"]
["TECHNIK","S0718310"]
["TECHNIK","S0718310.C"]
["TECHNIK","S0718330"]
["TECHNIK","S0718340"]
["TECHNIK","S0718440"]
["TECHNIK","S0718450"]
["TECHNIK","S0718450.C"]
["TECHNIK","S0718470"]
["TECHNIK","S0718500"]
["TECHNIK","S0718510"]
["TECHNIK","S0718520"]
["TECHNIK","S0718530"]
["TECHNIK","S0718580"]
["TECHNIK","S0718580.C"]
["TECHNIK","S0718600"]
["TECHNIK","S0718620"]
["TECHNIK","S0718860"]
["TECHNIK","S0719250"]
["TECHNIK","S0720160"]
["TECHNIK","S0720170"]
["TECHNIK","S0720180"]
["TECHNIK","S0720290"]
["TECHNIK","S0720300"]
["TECHNIK","S0720500"]
["TECHNIK","S0720510"]
["TECHNIK","S0720520"]
["TECHNIK","S0720530"]
["TECHNIK","S0720530.C"]
["TECHNIK","S0720540"]
["TECHNIK","S0720550"]
["TECHNIK","S0720560"]
["TECHNIK","S0720570"]
["TECHNIK","S0720580"]
["TECHNIK","S0720580.C"]
["TECHNIK","S0720590"]
["TECHNIK","S0720600"]
["TECHNIK","S0720610"]
["TECHNIK","S0720670"]
["TECHNIK","S0720670.C"]
["TECHNIK","S0720680"]
["TECHNIK","S0720680.C"]
["TECHNIK","S0720690"]
["TECHNIK","S0720700"]
["TECHNIK","S0720710"]
["TECHNIK","S0720720"]
["TECHNIK","S0720730"]
["TECHNIK","S0720730.C"]
["TECHNIK","S0720740"]
["TECHNIK","S0720770"]
["TECHNIK","S0720780"]
["TECHNIK","S0720790"]
["TECHNIK","S0720820"]
["TECHNIK","S0720830"]
["TECHNIK","S0720830.C"]
["TECHNIK","S0720840"]
["TECHNIK","S0720850"]
["TECHNIK","S0720860"]
["TECHNIK","S0720870"]
["TECHNIK","S0720880"]
["TECHNIK","S0720880.C"]
["TECHNIK","S0720890"]
["TECHNIK","S0720900"]
["TECHNIK","S0720910"]
["TECHNIK","S0720920"]
["TECHNIK","S0720930"]
["TECHNIK","S0720930.C"]
["TECHNIK","S0720940"]
["TECHNIK","S0720950"]
["TECHNIK","S0720960"]
["TECHNIK","S0720970"]
["TECHNIK","S0720980"]
["TECHNIK","S0720980.C"]
["TECHNIK","S0720990"]
["TECHNIK","S0721000"]
["TECHNIK","S0721010"]
["TECHNIK","S0721030"]
["TECHNIK","S0721090"]
["TECHNIK","S0721120"]
["TECHNIK","S0721140"]
["TECHNIK","S0721150"]
["TECHNIK","S0721180"]
["TECHNIK","S0721210"]
["TECHNIK","S0721250"]
["TECHNIK","S0721280"]
["TECHNIK","S0721300"]
["TECHNIK","S0721330"]
["TECHNIK","S0721500"]
["TECHNIK","S0721500.C"]
["TECHNIK","S0721540"]
["TECHNIK","S0721560"]
["TECHNIK","S0721560.C"]
["TECHNIK","S0721570"]
["TECHNIK","S0721570.C"]
["TECHNIK","S0721580"]
["TECHNIK","S0721590"]
["TECHNIK","S0721600"]
["TECHNIK","S0721710"]
["TECHNIK","S0721720"]
["TECHNIK","S0722370"]
["TECHNIK","S0722380"]
["TECHNIK","S0722400"]
["TECHNIK","S0722410"]
["TECHNIK","S0722430"]
["TECHNIK","S0722440"]
["TECHNIK","S0722460"]
["TECHNIK","S0722470"]
["TECHNIK","S0722480"]
["TECHNIK","S0722520"]
["TECHNIK","S0722530"]
["TECHNIK","S0722540"]
["TECHNIK","S0722550"]
["TECHNIK","S0722560"]
["TECHNIK","S0773830"]
["TECHNIK","S0773860"]
["TECHNIK","S0810090"]
["TECHNIK","S0810130"]
["TECHNIK","S0810170"]
["TECHNIK","S0810210"]
["TECHNIK","S0810330"]
["TECHNIK","S0847730"]
["TECHNIK","S0847740"]
["TECHNIK","S0847750"]
["TECHNIK","S0898130"]
["TECHNIK","S0898140"]
["TECHNIK","S0898150"]
["TECHNIK","S0898160"]
["TECHNIK","S0904980"]
["TECHNIK","S1805416"]
["TECHNIK","S1805417"]
["TECHNIK","S1805420"]
["TECHNIK","S1805422"]
["TECHNIK","S1805440"]
["TECHNIK","S1805443"]
["TECHNIK","S1805444"]
["TECHNIK SPECIAL - AKCIA","S700E"]
["TECHNIK","S700E nůž"]
["TECHNIK","S700E PÁS 6 bílá"]
["TECHNIK","S700E PÁS 6 stříbrná"]
["TECHNIK","S700E PÁS 6 žlutá"]
["TECHNIK","S700E PÁS 9 bílá"]
["TECHNIK","S700E PÁS 9 stříbrná"]
["TECHNIK","S700E PÁS 9 žlutá"]
["TECHNIK","S700E PÁS12 bílá"]
["TECHNIK","S700E PÁS12 stříbrná"]
["TECHNIK","S700E PÁS12 žlutá"]
["TECHNIK","S700E TISK černá"]
["TECHNIK","Sada PBF"]
["TECHNIK","Sada Phillips"]
["TECHNIK","Sada Pozidriv"]
["TECHNIK SPECIAL - AKCIA","SANITA 28,3 KPL"]
["TECHNIK SPECIAL - AKCIA","SANITA 28/32 KPL"]
["TECHNIK SPECIAL - AKCIA","SANITA 31,7 KPL"]
["TECHNIK SPECIAL - AKCIA","SANITA 35,0 KPL"]
["TECHNIK SPECIAL - AKCIA","SANITA SET"]
["TECHNIK SPECIAL - AKCIA","SANITA ŠROUB 10x55"]
["TECHNIK SPECIAL - AKCIA","SANITA ŠROUB M10x1"]
["TECHNIK SPECIAL - AKCIA","SC 05"]
["TECHNIK","SCORA  2"]
["TECHNIK","SCORA  2T"]
["TECHNIK","SCORA  6"]
["TECHNIK","SCORA  6T"]
["TECHNIK","SCORA  6Tsolar"]
["TECHNIK","SCORA  D"]
["TECHNIK","SCORA 10"]
["TECHNIK","SCORA 10P"]
["TECHNIK","SCORA 10T"]
["TECHNIK","SCORA 16"]
["TECHNIK","SCORA 16T"]
["TECHNIK","SCORA 25T"]
["TECHNIK","SCORA 35T"]
["TECHNIK","SCORA AWG 16-26"]
["TECHNIK","SCORA T"]
["TECHNIK","SI  0,5/PA"]
["TECHNIK","SI  1,5"]
["TECHNIK","SI  1,5/PA"]
["TECHNIK","SI  1,5/PA/T"]
["TECHNIK","SI  1,5/PC"]
["TECHNIK","SI  2,5"]
["TECHNIK","SI  2,5/1,5"]
["TECHNIK","SI  2,5/PA"]
["TECHNIK","SI  2,5/PA/T"]
["TECHNIK","SI  2,5/PC"]
["TECHNIK","SI  6"]
["TECHNIK","SI  6/1,5"]
["TECHNIK","SI  6/2,5"]
["TECHNIK","SI  6/32"]
["TECHNIK","SI  6/PA"]
["TECHNIK","SI  6/PA/T"]
["TECHNIK","SI  6/PC"]
["TECHNIK","SI 10"]
["TECHNIK","SI 10/6"]
["TECHNIK","SI 10/PA"]
["TECHNIK","SI 16"]
["TECHNIK","SI 16/10"]
["TECHNIK","SI 16/PA"]
["TECHNIK","SI 25"]
["TECHNIK","SI 25/PA"]
["TECHNIK","SI 35"]
["TECHNIK","SIK 1,5"]
["TECHNIK","SIK 2,5"]
["TECHNIK","SIK 6"]
["TECHNIK","Silikonový sprej"]
["TECHNIK","SIP 0,5/PA"]
["TECHNIK","SIP 1,5"]
["TECHNIK","SIP 1,5/PA"]
["TECHNIK","SIP 2,5"]
["TECHNIK","SIP 2,5/PA"]
["TECHNIK","SIP 6"]
["TECHNIK","SIP 6/PA"]
["TECHNIK","SIS 0,5"]
["TECHNIK","SIS 1,5"]
["TECHNIK","SIS 2,5"]
["TECHNIK","SIS 2,5/1,5"]
["TECHNIK","SIS 6"]
["TECHNIK","SIS 6/2,5"]
["TECHNIK","SIS10"]
["TECHNIK","SK 05"]
["TECHNIK","SK 06"]
["TECHNIK SPECIAL - AKCIA","SK 130"]
["TECHNIK SPECIAL - AKCIA","SK 130 PL"]
["TECHNIK SPECIAL - AKCIA","SK 130 U"]
["TECHNIK SPECIAL - AKCIA","SK 18"]
["TECHNIK SPECIAL - AKCIA","SK 22"]
["TECHNIK SPECIAL - AKCIA","SK 230"]
["TECHNIK SPECIAL - AKCIA","SK 50 PL"]
["TECHNIK SPECIAL - AKCIA","SK 520"]
["TECHNIK SPECIAL - AKCIA","SK 520 C"]
["TECHNIK","SK-COMBI NET"]
["TECHNIK","SK-KM"]
["TECHNIK","SK-KM-DI 054"]
["TECHNIK","SK-KM-DN 054"]
["TECHNIK","SK-KV"]
["TECHNIK","SK-LK1"]
["TECHNIK","SK-MOST 2"]
["TECHNIK SPECIAL - AKCIA","SKP 1"]
["TECHNIK SPECIAL - AKCIA","SKP 1 EL"]
["TECHNIK SPECIAL - AKCIA","SKP 1 MINI"]
["TECHNIK SPECIAL - AKCIA","SKP 1 NO"]
["TECHNIK","SK-PM"]
["TECHNIK","SK-PM-MO 056"]
["TECHNIK","SK-PM-MOC 056"]
["TECHNIK","SK-PROFI CRIMP"]
["TECHNIK","SK-PROFI CRIMP NET"]
["TECHNIK","SK-PV"]
["TECHNIK","SK-PV-OI 056"]
["TECHNIK","SK-PV-ON 056"]
["TECHNIK","SK-SOLAR H&S"]
["TECHNIK","SK-SOLAR MC"]
["TECHNIK","SK-SOLAR TYCO"]
["TECHNIK","SK-SOLAR UNI"]
["TECHNIK","SK-TF"]
["TECHNIK","SK-TF 5"]
["TECHNIK","SK-TF PLUS"]
["TECHNIK","SK-TF PLUS 5"]
["TECHNIK","SL  0,5"]
["TECHNIK","SL  0,75"]
["TECHNIK","SL  1,5"]
["TECHNIK","SL  1,5/20"]
["TECHNIK","SL  1,5/25"]
["TECHNIK","SL  2,5"]
["TECHNIK","SL  2,5/20"]
["TECHNIK","SL  2,5/25"]
["TECHNIK","SL  4-6"]
["TECHNIK","SL  4-6/20"]
["TECHNIK","SL  6"]
["TECHNIK","SL  6/25"]
["TECHNIK","SL 10"]
["TECHNIK","SL 16"]
["TECHNIK","SL 25"]
["TECHNIK","SL 35"]
["TECHNIK","SL 50"]
["TECHNIK","SL 70"]
["TECHNIK","SL 95"]
["TECHNIK","SL120"]
["TECHNIK","SL150"]
["TECHNIK","SL185"]
["TECHNIK","SL240"]
["TECHNIK","SL300"]
["TECHNIK","SL400"]
["TECHNIK","SL500"]
["TECHNIK","SLN  1,5"]
["TECHNIK","SLN  2,5"]
["TECHNIK","SLN  6"]
["TECHNIK","SLN 16"]
["TECHNIK","SLP  0,5"]
["TECHNIK","SLP  0,5/5"]
["TECHNIK","SLP  1,5"]
["TECHNIK","SLP  1,5/6"]
["TECHNIK","SLP  2,5"]
["TECHNIK","SLP  2,5/6"]
["TECHNIK","SLP  4-6"]
["TECHNIK","SLP  4-6/6"]
["TECHNIK","SLP 10"]
["TECHNIK","SLP 10/8"]
["TECHNIK","SLP 16"]
["TECHNIK","SLP 16/10"]
["TECHNIK","SLP 25"]
["TECHNIK","SLP 35"]
["TECHNIK","SLP 50"]
["TECHNIK","SLP 70"]
["TECHNIK","SLP 95"]
["TECHNIK","SLP120"]
["TECHNIK","SLV   1,5 CU/3"]
["TECHNIK","SLV   1,5 CU/5"]
["TECHNIK","SLV   2,5 CU/3"]
["TECHNIK","SLV   2,5 CU/5"]
["TECHNIK","SLV   2,5-10"]
["TECHNIK","SLV   4,0 CU/5"]
["TECHNIK","SLV   6,0 CU/5"]
["TECHNIK","SLV   6-25"]
["TECHNIK","SLV   6-25/5"]
["TECHNIK","SLV  10 AL"]
["TECHNIK","SLV  10 CU/5"]
["TECHNIK","SLV  16 AL"]
["TECHNIK","SLV  16 AL/5"]
["TECHNIK","SLV  16 CU"]
["TECHNIK","SLV  16 CU/5"]
["TECHNIK","SLV  16-70"]
["TECHNIK","SLV  25 AL"]
["TECHNIK","SLV  25 AL/5"]
["TECHNIK","SLV  25 CU"]
["TECHNIK","SLV  25 CU/5"]
["TECHNIK","SLV  35 AL"]
["TECHNIK","SLV  35 CU"]
["TECHNIK","SLV  35 CU/5"]
["TECHNIK","SLV  35-185"]
["TECHNIK","SLV  50 AL"]
["TECHNIK","SLV  50 CU"]
["TECHNIK","SLV  70 AL"]
["TECHNIK","SLV  70 CU"]
["TECHNIK","SLV  95 AL"]
["TECHNIK","SLV  95 CU"]
["TECHNIK","SLV 120 AL"]
["TECHNIK","SLV 120 CU"]
["TECHNIK","SLV 120-240"]
["TECHNIK","SLV 150 AL"]
["TECHNIK","SLV 150 CU"]
["TECHNIK","SLV 185 AL"]
["TECHNIK","SLV 185 CU"]
["TECHNIK","SLV 240 AL"]
["TECHNIK","SLV 240 CU"]
["TECHNIK","SLV 240/1x120"]
["TECHNIK","SLV-SV  1,5-6"]
["TECHNIK","SLV-SV  1,5-6/5"]
["TECHNIK","SLV-SV  2,5"]
["TECHNIK","SLV-SV  2,5/5"]
["TECHNIK","SLV-SV  4"]
["TECHNIK","SLV-SV  4/5"]
["TECHNIK","SLV-SV  4-16"]
["TECHNIK","SLV-SV  4-16/5"]
["TECHNIK","SLV-SV  6"]
["TECHNIK","SLV-SV  6/5"]
["TECHNIK","SLV-SV  6-25"]
["TECHNIK","SLV-SV  6-25/5"]
["TECHNIK","SLV-SV  6-25/5T"]
["TECHNIK","SLV-SV  6-25/T"]
["TECHNIK","SLV-SV 10"]
["TECHNIK","SLV-SV 10/5"]
["TECHNIK","SLV-SV 16-50"]
["TECHNIK","SLV-SV 35- 95"]
["TECHNIK","SLV-SV 35-150"]
["TECHNIK","SLV-SV 35-185"]
["TECHNIK","SLV-SV 95-240"]
["TECHNIK","SLV-SV120-240"]
["TECHNIK","SLV-SV120-240 AL"]
["TECHNIK","SLV-SV150-240"]
["TECHNIK","SLV-SV150-240 AL"]
["TECHNIK","SLV-SV3x240/120 AL"]
["TECHNIK","SN 2"]
["TECHNIK","SPB  4"]
["TECHNIK","SPB  6"]
["TECHNIK","SPB  8"]
["TECHNIK","SPB 10"]
["TECHNIK","SPB 12"]
["TECHNIK","SPB 15"]
["TECHNIK","SPB 20"]
["TECHNIK","SPC  2"]
["TECHNIK","SPC  4"]
["TECHNIK","SPC  6"]
["TECHNIK","SPC  8"]
["TECHNIK","SPC 10"]
["TECHNIK","SPC 12"]
["TECHNIK","SPC 15"]
["TECHNIK","SPC 20"]
["TECHNIK SPECIAL - AKCIA","SPÍNAČ NOŽNÍ"]
["TECHNIK","SPO  2"]
["TECHNIK","SPO  4"]
["TECHNIK","SPO 10"]
["TECHNIK","SPP  2"]
["TECHNIK","SPP  4"]
["TECHNIK","SPP  6"]
["TECHNIK","SPP  8"]
["TECHNIK","SPP 10"]
["TECHNIK","SPP 12"]
["TECHNIK","SPP 15"]
["TECHNIK","SPP 20"]
["TECHNIK","SPR  4 PVC"]
["TECHNIK","Sprej na řetězy,lana"]
["TECHNIK","SR  2,5x 80"]
["TECHNIK","SR  3,0x100"]
["TECHNIK","SR  3,5x100"]
["TECHNIK","SR  4,0x100"]
["TECHNIK","SR  5,5 SET"]
["TECHNIK","SR  5,5x125"]
["TECHNIK","SR  6,5 SET"]
["TECHNIK","SR  6,5x150"]
["TECHNIK","SR  8,0x175"]
["TECHNIK","SR 10 SET"]
["TECHNIK","SR 10x200"]
["TECHNIK","SR PH 0"]
["TECHNIK","SR PH 0-4 SET"]
["TECHNIK","SR PH 1"]
["TECHNIK","SR PH 1-3 SET"]
["TECHNIK","SR PH 1-4 SET"]
["TECHNIK","SR PH 2"]
["TECHNIK","SR PH 3"]
["TECHNIK","SR PH 4"]
["TECHNIK","SR PZ 0"]
["TECHNIK","SR PZ 0-4 SET"]
["TECHNIK","SR PZ 1"]
["TECHNIK","SR PZ 1-3 SET"]
["TECHNIK","SR PZ 1-4 SET"]
["TECHNIK","SR PZ 2"]
["TECHNIK","SR PZ 3"]
["TECHNIK","SR PZ 4"]
["TECHNIK","SR TX10"]
["TECHNIK","SR TX15"]
["TECHNIK","SR TX25"]
["TECHNIK","SR TX27"]
["TECHNIK","SR TX30"]
["TECHNIK","ST 1100 T"]
["TECHNIK","ST 200 T"]
["TECHNIK","ST 2200 T"]
["TECHNIK","ST 2200 T hrot"]
["TECHNIK","ST 250 K"]
["TECHNIK","ST kombi 1"]
["TECHNIK","ST kombi 2"]
["TECHNIK SPECIAL - AKCIA","STANDARD 12,7 KPL"]
["TECHNIK SPECIAL - AKCIA","STANDARD 16,2 KPL"]
["TECHNIK SPECIAL - AKCIA","STANDARD 20,4 KPL"]
["TECHNIK SPECIAL - AKCIA","STANDARD 22,5 KPL"]
["TECHNIK SPECIAL - AKCIA","STANDARD 25,4 KPL"]
["TECHNIK SPECIAL - AKCIA","STANDARD 28,3 KPL"]
["TECHNIK SPECIAL - AKCIA","STANDARD 30,5 KPL"]
["TECHNIK SPECIAL - AKCIA","STANDARD 42,8 KPL"]
["TECHNIK SPECIAL - AKCIA","STANDARD 65,0"]
["TECHNIK SPECIAL - AKCIA","STANDARD 68,0 KPL"]
["TECHNIK SPECIAL - AKCIA","STANDARD 70,0 KPL"]
["TECHNIK SPECIAL - AKCIA","STANDARD 75,5 KPL"]
["TECHNIK SPECIAL - AKCIA","STANDARD 76,2 KPL"]
["TECHNIK SPECIAL - AKCIA","STANDARD 80,0 KPL"]
["TECHNIK SPECIAL - AKCIA","STANDARD 82,0 KPL"]
["TECHNIK SPECIAL - AKCIA","STANDARD 89,0"]
["TECHNIK SPECIAL - AKCIA","STANDARD 92,0"]
["TECHNIK SPECIAL - AKCIA","STANDARD SET Pg 7-48"]
["TECHNIK SPECIAL - AKCIA","STANDARD100,5"]
["TECHNIK SPECIAL - AKCIA","STANDARD120,0"]
["TECHNIK","ST-HG 1"]
["TECHNIK","ST-MPH"]
["TECHNIK","Stojan PBF"]
["TECHNIK","ST-RFR PIEZO"]
["TECHNIK","STRIPAX 1"]
["TECHNIK","STRIPAX 10"]
["TECHNIK","STRIPAX 16"]
["TECHNIK","STRIPAX 6"]
["TECHNIK","STRIPAX 6H"]
["TECHNIK","STRIPAX 6UL"]
["TECHNIK","STRIPAX PLUS"]
["TECHNIK","STRIPIT 12"]
["TECHNIK","STRIPIT 16"]
["TECHNIK","STRIPIT 6"]
["TECHNIK","SU  1,5"]
["TECHNIK","SU  2,5"]
["TECHNIK","SU  6"]
["TECHNIK","SU 10"]
["TECHNIK","SVCZV  3x1,5-2,5"]
["TECHNIK","SVCZV  4x1,5-2,5"]
["TECHNIK","SVCZV  4x4-6"]
["TECHNIK","SVCZV  5x1,5-2,5"]
["TECHNIK","SVCZV  5x4-6"]
["TECHNIK","SVCZV  7x1,5-2,5"]
["TECHNIK","SVCZV  7x4-6"]
["TECHNIK","SVCZV 12x0,5-1"]
["TECHNIK","SVCZV 12x1,5-2,5"]
["TECHNIK","SVCZV 12x4-6"]
["TECHNIK","SVCZV 19x1,5-2,5"]
["TECHNIK","SVCZV 24x0,5-1"]
["TECHNIK","SVCZV 37x1,5-2,5"]
["TECHNIK","SZ  1,0-2,5"]
["TECHNIK","SZ  1,5-3,5"]
["TECHNIK","SZ  1,5-5"]
["TECHNIK","SZ  3-9"]
["TECHNIK","SZ  4-16"]
["TECHNIK","SZ 10-21"]
["TECHNIK","SZT  1,5-10"]
["TECHNIK","SZT  4-21"]
["TECHNIK","SZT 10-30"]
["TECHNIK","Šok na rez"]
["TECHNIK SPECIAL - AKCIA","ŠROUB  6x40"]
["TECHNIK SPECIAL - AKCIA","ŠROUB  9,5x50"]
["TECHNIK SPECIAL - AKCIA","ŠROUB 11,1x60"]
["TECHNIK SPECIAL - AKCIA","ŠROUB 19x55"]
["TECHNIK SPECIAL - AKCIA","ŠROUB 19x75"]
["TECHNIK SPECIAL - AKCIA","ŠROUB BL  9,5x50"]
["TECHNIK SPECIAL - AKCIA","TC 025"]
["TECHNIK SPECIAL - AKCIA","TC 04"]
["TECHNIK SPECIAL - AKCIA","TC 045"]
["TECHNIK SPECIAL - AKCIA","TC 050"]
["TECHNIK SPECIAL - AKCIA","TC 055"]
["TECHNIK SPECIAL - AKCIA","TC 085"]
["TECHNIK SPECIAL - AKCIA","TC 096"]
["TECHNIK SPECIAL - AKCIA","TC 120"]
["TECHNIK SPECIAL - AKCIA","TC 120 kufr"]
["TECHNIK","TC-201"]
["TECHNIK","TC-291"]
["TECHNIK","TC-491"]
["TECHNIK","TC-495"]
["TECHNIK","TC-591"]
["TECHNIK","TC-601"]
["TECHNIK","TC-691"]
["TECHNIK","Teflonový sprej"]
["TECHNIK","TFL 12x10"]
["REIKU-B","TKBSB- 7,5"]
["REIKU-B","TKBSB-10"]
["REIKU-B","TKBSB-12,5"]
["REIKU-B","TKBSB-14"]
["REIKU-B","TKBSB-15,5"]
["REIKU-B","TKBSB-19,5"]
["REIKU-B","TKBSB-22"]
["REIKU-B","TKBSB-28"]
["REIKU-B","TKKSB 70B14"]
["REIKU-B","TKKSB23BLIND"]
["REIKU-B","TKKSB29BLIND"]
["REIKU-B","TKKSB-36B01"]
["REIKU-B","TKKSB36BLIND"]
["REIKU-B","TKKSB42BLIND"]
["REIKU-B","TKKSB-48B01"]
["REIKU-B","TKKSB48BLIND"]
["REIKU-B","TKKSB-52B01"]
["REIKU-B","TKKSB-52B02"]
["REIKU-B","TKKSB52BLIND"]
["REIKU-B","TKKSB-70B01"]
["REIKU-B","TKKSB-70B02"]
["REIKU-B","TKKSB-70B03"]
["REIKU-B","TKKSB-70B04"]
["REIKU-B","TKKSB-70B05"]
["REIKU-B","TKKSB-70B06"]
["REIKU-B","TKKSB-70B07"]
["REIKU-B","TKKSB-70B12"]
["REIKU-B","TKKSB-70B13"]
["REIKU-B","TKKSB70BLIND"]
["TECHNIK","TKT  25"]
["TECHNIK","TKT  50"]
["TECHNIK","TKT  75"]
["TECHNIK","TKT 100"]
["TECHNIK","TKT 150"]
["TECHNIK","Tlakový vzduch"]
["TECHNIK SPECIAL - AKCIA","TM-3000"]
["TECHNIK SPECIAL - AKCIA","TM-EVFJ1"]
["TECHNIK","TM-K231"]
["TECHNIK","TN  70 SE"]
["TECHNIK","TN 120 SE"]
["TECHNIK","TNN  70"]
["TECHNIK","TNN 120"]
["TECHNIK","TO 4040052"]
["TECHNIK","TO 4060045"]
["TECHNIK","Tool Box"]
["TECHNIK SPECIAL - AKCIA","TOOL SET 11"]
["TECHNIK SPECIAL - AKCIA","TOOL SET 12"]
["TECHNIK","Top - Lub"]
["TECHNIK SPECIAL - AKCIA","TP76E"]
["TECHNIK SPECIAL - AKCIA","TP80E"]
["TECHNIK","TP80E nůž"]
["TECHNIK","TP80E PÁS 6 bílá"]
["TECHNIK","TP80E PÁS 6 stříbrná"]
["TECHNIK","TP80E PÁS 6 žlutá"]
["TECHNIK","TP80E PÁS 9 bílá"]
["TECHNIK","TP80E PÁS 9 stříbrná"]
["TECHNIK","TP80E PÁS 9 žlutá"]
["TECHNIK","TP80E PÁS12 bílá"]
["TECHNIK","TP80E PÁS12 stříbrná"]
["TECHNIK","TP80E PÁS12 žlutá"]
["TECHNIK","TP80E TISK černá"]
["REIKU-B","TPDVW-07"]
["REIKU-B","TPDVW-10"]
["REIKU-B","TPDVW-12"]
["REIKU-B","TPDVW-17"]
["REIKU-B","TPDVW-23"]
["REIKU-B","TPDVW-29"]
["REIKU-B","TPDVW-36"]
["REIKU-B","TPDVW-48"]
["REIKU-B","TPRIB-10F"]
["REIKU-B","TPRIB-12F"]
["REIKU-B","TPRIB-17F"]
["REIKU-B","TPRIB-23F"]
["REIKU-B","TPRIB-29F"]
["REIKU-B","TPRIB-36M"]
["REIKU-B","TPRIB-48M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 12,5"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 12,5 KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 12,5 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 12,5 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 15,2"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 15,2 KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 15,2 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 15,2 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 16,2"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 16,2 KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 16,2 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 16,2 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 18,6"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 18,6 KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 18,6 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 18,6 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 20,4"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 20,4 KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 20,4 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 20,4 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 22,5"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 22,5 KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 22,5 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 22,5 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 25,4"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 25,4 KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 25,4 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 25,4 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 28,3"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 28,3 KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 28,3 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 28,3 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 30,5"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 30,5 KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 30,5 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 30,5 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 32,5"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 32,5 KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 32,5 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 32,5 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 37,0"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 37,0 KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 37,0 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 37,0 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 40,5"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 40,5 KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 40,5 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 40,5 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 43,2"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 47,0"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 47,0 KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 47,0 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 47,0 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 50,5"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 50,5 KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 50,5 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 50,5 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 54,0"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 54,0 KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 54,0 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 54,0 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 60,0"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 60,0 KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 60,0 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 60,0 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 63,5"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 63,5 KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 63,5 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR 63,5 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 15,2"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 15,2 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 15,2 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 15,2KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 16,2"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 16,2 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 16,2 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 16,2KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 18,6"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 18,6 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 18,6 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 18,6KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 20,4"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 20,4 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 20,4 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 20,4KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 22,5"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 22,5 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 22,5 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 22,5KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 25,4"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 25,4 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 25,4 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 25,4KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 28,3"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 28,3 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 28,3 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 28,3KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 30,5"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 30,5 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 30,5 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 30,5KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 32,5"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 32,5 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 32,5 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 32,5KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 37,0"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 37,0 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 37,0 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 37,0KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 40,5"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 40,5 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 40,5 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 40,5KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 47,0"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 47,0 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 47,0 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 47,0KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 50,5"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 50,5KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 54,0"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 54,0 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 54,0 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 54,0KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 60,0"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 60,0 M"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 60,0 R"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 60,0KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 63,5"]
["TECHNIK SPECIAL - AKCIA","TRISTAR PLUS 63,5KPL"]
["TECHNIK SPECIAL - AKCIA","TRISTAR SET M12-40"]
["TECHNIK SPECIAL - AKCIA","TRISTAR SET M16-63"]
["TECHNIK SPECIAL - AKCIA","TRISTAR SET M16-63 L"]
["TECHNIK SPECIAL - AKCIA","TRISTAR SET Pg 9-21"]
["TECHNIK SPECIAL - AKCIA","TRISTAR SET Pg 9-48"]
["TECHNIK SPECIAL - AKCIA","TRISTAR SET+ M16-40"]
["TECHNIK SPECIAL - AKCIA","TRISTAR SET+ M16-63"]
["TECHNIK SPECIAL - AKCIA","TRISTAR SET+ Pg 9-21"]
["TECHNIK SPECIAL - AKCIA","TRISTAR SET+ Pg 9-48"]
["TECHNIK","TRITEST eazy"]
["TECHNIK","TRITEST PRO"]
["TECHNIK SPECIAL - AKCIA","TRS-B70"]
["TECHNIK","TS 0"]
["TECHNIK","TS 1"]
["TECHNIK","TS 12"]
["TECHNIK","TS 2"]
["TECHNIK","TS 22"]
["TECHNIK","TS 3"]
["TECHNIK","TS 3000T"]
["TECHNIK","TS 4000T"]
["TECHNIK","TS 5"]
["TECHNIK","TS 51"]
["TECHNIK","TS 6"]
["TECHNIK","TS 61"]
["TECHNIK","TS 7000T"]
["TECHNIK","TS 8000BT"]
["TECHNIK","TS 839T"]
["TECHNIK","Tuk ve spreji"]
["TECHNIK","TWISTER 341"]
["TECHNIK","TWISTER 342"]
["TECHNIK","TWISTER 344 PRO"]
["TECHNIK","TX 221"]
["TECHNIK","TX 231"]
["TECHNIK","TX 241"]
["TECHNIK","TX 251"]
["TECHNIK","TX 621"]
["TECHNIK","TX 631"]
["TECHNIK","TX9"]
["TECHNIK","TZe 111"]
["TECHNIK","TZe 121"]
["TECHNIK","TZe 131"]
["TECHNIK","TZe 132"]
["TECHNIK","TZe 141"]
["TECHNIK","TZe 151"]
["TECHNIK","TZe 161"]
["TECHNIK","TZe 211"]
["TECHNIK","TZe 211.C"]
["TECHNIK","TZe 221"]
["TECHNIK","TZe 221.C"]
["TECHNIK","TZe 222"]
["TECHNIK","TZe 231"]
["TECHNIK","TZe 231.C"]
["TECHNIK","TZe 241"]
["TECHNIK","TZe 241.C"]
["TECHNIK","TZe 251"]
["TECHNIK","TZe 251.C"]
["TECHNIK","TZe 261"]
["TECHNIK","TZe 262"]
["TECHNIK","TZe 315"]
["TECHNIK","TZe 325"]
["TECHNIK","TZe 335"]
["TECHNIK","TZe 345"]
["TECHNIK","TZe 355"]
["TECHNIK","TZe 421"]
["TECHNIK","TZe 431"]
["TECHNIK","TZe 441"]
["TECHNIK","TZe 451"]
["TECHNIK","TZe 461"]
["TECHNIK","TZe 521"]
["TECHNIK","TZe 531"]
["TECHNIK","TZe 535"]
["TECHNIK","TZe 551"]
["TECHNIK","TZe 611"]
["TECHNIK","TZe 611.C"]
["TECHNIK","TZe 621"]
["TECHNIK","TZe 621.C"]
["TECHNIK","TZe 631"]
["TECHNIK","TZe 631.C"]
["TECHNIK","TZe 641"]
["TECHNIK","TZe 641.C"]
["TECHNIK","TZe 651"]
["TECHNIK","TZe 651.C"]
["TECHNIK","TZe 661"]
["TECHNIK","TZe 721"]
["TECHNIK","TZe 731"]
["TECHNIK","TZe 741"]
["TECHNIK","TZe B31"]
["TECHNIK","TZe C51"]
["TECHNIK","TZe FX231"]
["TECHNIK","TZe FX241"]
["TECHNIK","TZe FX251"]
["TECHNIK","TZe FX621"]
["TECHNIK","TZe FX641"]
["TECHNIK","TZe FX651"]
["TECHNIK","TZe M931"]
["TECHNIK","TZe M961"]
["TECHNIK","TZe N221"]
["TECHNIK","TZe N231"]
["TECHNIK","TZe N241"]
["TECHNIK","TZe S211"]
["TECHNIK","TZe S211.C"]
["TECHNIK","TZe S221"]
["TECHNIK","TZe S221.C"]
["TECHNIK","TZe S231"]
["TECHNIK","TZe S231.C"]
["TECHNIK","TZe S241"]
["TECHNIK","TZe S241.C"]
["TECHNIK","TZe S251"]
["TECHNIK","TZe S251.C"]
["TECHNIK","TZe S261"]
["TECHNIK","TZe S261.C"]
["TECHNIK","TZe S611.C"]
["TECHNIK","TZe S621"]
["TECHNIK","TZe S631"]
["TECHNIK","TZe S641"]
["TECHNIK","TZe S651"]
["TECHNIK","TZe SE4"]
["TECHNIK","UB 2A"]
["TECHNIK","UK-2 AAA akce"]
["TECHNIK","UK-4 AA"]
["TECHNIK","UL 100-E SET"]
["TECHNIK SPECIAL - AKCIA","UNIC-G"]
["TECHNIK SPECIAL - AKCIA","UNIC-L"]
["TECHNIK SPECIAL - AKCIA","UNIC-LS"]
["TECHNIK SPECIAL - AKCIA","UNIC-LZ"]
["TECHNIK SPECIAL - AKCIA","UNICUT 8"]
["TECHNIK","UNISET black"]
["TECHNIK","UNISET color"]
["TECHNIK","UNISET PBF"]
["TECHNIK","UR 2"]
["TECHNIK","Ušlechtilá ocel"]
["TECHNIK","Uvolňovací sprej"]
["TECHNIK","Uvolňovač šroubů"]
["TECHNIK","UY"]
["TECHNIK","UY 2"]
["TECHNIK SPECIAL - AKCIA","V 24/230 UNI-F"]
["REIKU-B","V2 connector NW07"]
["REIKU-B","V2 connector NW10"]
["REIKU-B","V2 connector NW12"]
["REIKU-B","V2 connector NW17"]
["REIKU-B","V2 connector NW23"]
["REIKU-B","V2 connector NW29"]
["TECHNIK","VA 1000"]
["REIKU-B","VAKEM"]
["REIKU-B","VAKEM-1.5"]
["REIKU-B","Variable REIKU distribution piece, Basic piece for sizes NW07-NW17"]
["TECHNIK","VFP  80x100 žl-černá"]
["TECHNIK","VFP 100x100 žl-černá"]
["TECHNIK","VI  0,5-M 2/PA"]
["TECHNIK","VI  0,5-M 3,5/PA"]
["TECHNIK","VI  0,5-M 3/PA"]
["TECHNIK","VI  0,5-M 4/PA"]
["TECHNIK","VI  0,5-M 5/PA"]
["TECHNIK","VI  1,5-M 3"]
["TECHNIK","VI  1,5-M 3,5"]
["TECHNIK","VI  1,5-M 3,5/E"]
["TECHNIK","VI  1,5-M 3,5/PA"]
["TECHNIK","VI  1,5-M 3,5/PC"]
["TECHNIK","VI  1,5-M 3/E"]
["TECHNIK","VI  1,5-M 3/PA"]
["TECHNIK","VI  1,5-M 3/PC"]
["TECHNIK","VI  1,5-M 4"]
["TECHNIK","VI  1,5-M 4/8"]
["TECHNIK","VI  1,5-M 4/8/PA"]
["TECHNIK","VI  1,5-M 4/PA"]
["TECHNIK","VI  1,5-M 4/PC"]
["TECHNIK","VI  1,5-M 5"]
["TECHNIK","VI  1,5-M 5/10"]
["TECHNIK","VI  1,5-M 5/E"]
["TECHNIK","VI  1,5-M 5/PA"]
["TECHNIK","VI  1,5-M 5/PC"]
["TECHNIK","VI  1,5-M 6"]
["TECHNIK","VI  1,5-M 6/10"]
["TECHNIK","VI  1,5-M 6/E"]
["TECHNIK","VI  1,5-M 6/PA"]
["TECHNIK","VI  1,5-M 6/PC"]
["TECHNIK","VI  1,5-M 8"]
["TECHNIK","VI  1,5-M10"]
["TECHNIK","VI  1,5-M12"]
["TECHNIK","VI  2,5-M 3"]
["TECHNIK","VI  2,5-M 3,5"]
["TECHNIK","VI  2,5-M 3,5/E"]
["TECHNIK","VI  2,5-M 3,5/PA"]
["TECHNIK","VI  2,5-M 3,5/PC"]
["TECHNIK","VI  2,5-M 3/E"]
["TECHNIK","VI  2,5-M 3/PA"]
["TECHNIK","VI  2,5-M 3/PC"]
["TECHNIK","VI  2,5-M 4"]
["TECHNIK","VI  2,5-M 4/6"]
["TECHNIK","VI  2,5-M 4/8"]
["TECHNIK","VI  2,5-M 4/E"]
["TECHNIK","VI  2,5-M 4/PA"]
["TECHNIK","VI  2,5-M 4/PC"]
["TECHNIK","VI  2,5-M 5"]
["TECHNIK","VI  2,5-M 5/10"]
["TECHNIK","VI  2,5-M 5/10/E"]
["TECHNIK","VI  2,5-M 5/10/PA"]
["TECHNIK","VI  2,5-M 5/10/PC"]
["TECHNIK","VI  2,5-M 5/10/PK"]
["TECHNIK","VI  2,5-M 6"]
["TECHNIK","VI  2,5-M 6/10"]
["TECHNIK","VI  2,5-M 6/E"]
["TECHNIK","VI  2,5-M 6/PA"]
["TECHNIK","VI  2,5-M 6/PC"]
["TECHNIK","VI  2,5-M 8"]
["TECHNIK","VI  2,5-M10"]
["TECHNIK","VI  2,5-M12"]
["TECHNIK","VI  6-M 3"]
["TECHNIK","VI  6-M 3,5"]
["TECHNIK","VI  6-M 3,5/E"]
["TECHNIK","VI  6-M 3,5/PA"]
["TECHNIK","VI  6-M 3,5/PC"]
["TECHNIK","VI  6-M 3/E"]
["TECHNIK","VI  6-M 4"]
["TECHNIK","VI  6-M 4/10"]
["TECHNIK","VI  6-M 4/7"]
["TECHNIK","VI  6-M 4/7/E"]
["TECHNIK","VI  6-M 4/8/PC"]
["TECHNIK","VI  6-M 4/E"]
["TECHNIK","VI  6-M 4/PA"]
["TECHNIK","VI  6-M 5"]
["TECHNIK","VI  6-M 5/E"]
["TECHNIK","VI  6-M 5/PA"]
["TECHNIK","VI  6-M 5/PC"]
["TECHNIK","VI  6-M 6"]
["TECHNIK","VI  6-M 6/E"]
["TECHNIK","VI  6-M 6/PA"]
["TECHNIK","VI  6-M 6/PC"]
["TECHNIK","VI  6-M 8"]
["TECHNIK","VI  6-M 8/E"]
["TECHNIK","VI  6-M 8/PA"]
["TECHNIK","VI  6-M 8/PC"]
["TECHNIK","VI  6-M10"]
["TECHNIK","VI  6-M10/PA"]
["TECHNIK","VI  6-M10/PC"]
["TECHNIK","VI  6-M12"]
["TECHNIK","VI  6-M16"]
["TECHNIK","VI 10-M 4/PA"]
["TECHNIK","VI 10-M 5/PA"]
["TECHNIK","VI 10-M 6/PA"]
["TECHNIK","VI 10-M 8/PA"]
["TECHNIK","VI 10-M10/PA"]
["TECHNIK","VI 16-M 4/PA"]
["TECHNIK","VI 16-M 5/PA"]
["TECHNIK","VI 16-M 6/PA"]
["TECHNIK","VI 16-M 8/PA"]
["TECHNIK","VIF  1,5-M 4"]
["TECHNIK","VIF  1,5-M 5"]
["TECHNIK","VIF  2,5-M 4"]
["TECHNIK","VIF  2,5-M 5"]
["TECHNIK","VIF  6-M 4"]
["TECHNIK","VIF  6-M 5"]
["TECHNIK","VIS 1,5-M 3"]
["TECHNIK","VIS 1,5-M 3,5"]
["TECHNIK","VIS 1,5-M 4"]
["TECHNIK","VIS 1,5-M 4/7"]
["TECHNIK","VIS 1,5-M 5"]
["TECHNIK","VIS 1,5-M 6"]
["TECHNIK","VIS 2,5-M 3"]
["TECHNIK","VIS 2,5-M 3,5"]
["TECHNIK","VIS 2,5-M 4"]
["TECHNIK","VIS 2,5-M 4/7"]
["TECHNIK","VIS 2,5-M 5"]
["TECHNIK","VIS 2,5-M 5/8"]
["TECHNIK","VIS 2,5-M 6"]
["TECHNIK","VIS 6-M 3"]
["TECHNIK","VIS 6-M 3,5"]
["TECHNIK","VIS 6-M 4"]
["TECHNIK","VIS 6-M 5"]
["TECHNIK","VIS 6-M 6"]
["TECHNIK","VIS 6-M 8"]
["TECHNIK","VIS 6-M10"]
["TECHNIK","VK  3-14"]
["TECHNIK","VK  4-30"]
["TECHNIK","VK  8-20"]
["TECHNIK","VK 16"]
["TECHNIK","VK 16 DL"]
["TECHNIK","VK 16-30"]
["TECHNIK","VK 20"]
["TECHNIK","VK 20 DL"]
["TECHNIK","VK 24"]
["TECHNIK","VK 26"]
["TECHNIK","VK 26 DL"]
["TECHNIK","VK 26-40"]
["TECHNIK","VK 36-50"]
["TECHNIK","VK 46-60"]
["TECHNIK SPECIAL - AKCIA","VKS 125"]
["TECHNIK SPECIAL - AKCIA","VKS 125 břit"]
["TECHNIK SPECIAL - AKCIA","VKS 125 džák"]
["REIKU-B","VMARB-10M16"]
["REIKU-B","VMARB-10M20"]
["REIKU-B","VMARB-10P09"]
["REIKU-B","VMARB-12M16"]
["REIKU-B","VMARB-12M20"]
["REIKU-B","VMARB-12P11"]
["REIKU-B","VMARB-17M20"]
["REIKU-B","VMARB-17M25"]
["REIKU-B","VMARB-17P13"]
["REIKU-B","VMARB-17P16"]
["REIKU-B","VMARB-23M32"]
["REIKU-B","VMARB-23P21"]
["REIKU-B","VMARB-29M32"]
["REIKU-B","VMARB-29M40"]
["REIKU-B","VMARB-29P29"]
["REIKU-B","VMARB-36M40"]
["REIKU-B","VMARB-36M50"]
["REIKU-B","VMARB-36P36"]
["REIKU-B","VMARB-48M63"]
["REIKU-B","VMARB-48P48"]
["REIKU-G","VMARG-10M16"]
["REIKU-G","VMARG-10M20"]
["REIKU-G","VMARG-10P09"]
["REIKU-G","VMARG-12M16"]
["REIKU-G","VMARG-12M20"]
["REIKU-G","VMARG-12P11"]
["REIKU-G","VMARG-17M20"]
["REIKU-G","VMARG-17M25"]
["REIKU-G","VMARG-17P13"]
["REIKU-G","VMARG-17P16"]
["REIKU-G","VMARG-23M32"]
["REIKU-G","VMARG-23P21"]
["REIKU-G","VMARG-29M32"]
["REIKU-G","VMARG-29M40"]
["REIKU-G","VMARG-29P29"]
["REIKU-G","VMARG-36M40"]
["REIKU-G","VMARG-36M50"]
["REIKU-G","VMARG-36P36"]
["REIKU-G","VMARG-48M63"]
["REIKU-G","VMARG-48P48"]
["REIKU-B","VMAVB-10M16"]
["REIKU-B","VMAVB-10M20"]
["REIKU-B","VMAVB-10P09"]
["REIKU-B","VMAVB-12M16"]
["REIKU-B","VMAVB-12M20"]
["REIKU-B","VMAVB-12P11"]
["REIKU-B","VMAVB-17M20"]
["REIKU-B","VMAVB-17M25"]
["REIKU-B","VMAVB-17P13"]
["REIKU-B","VMAVB-17P16"]
["REIKU-B","VMAVB-23M32"]
["REIKU-B","VMAVB-23P21"]
["REIKU-B","VMAVB-29M32"]
["REIKU-B","VMAVB-29M40"]
["REIKU-B","VMAVB-29P29"]
["REIKU-B","VMAVB-36M40"]
["REIKU-B","VMAVB-36M50"]
["REIKU-B","VMAVB-36P36"]
["REIKU-B","VMAVB-48M63"]
["REIKU-B","VMAVB-48P48"]
["REIKU-G","VMAVG-10M16"]
["REIKU-G","VMAVG-10M20"]
["REIKU-G","VMAVG-10P09"]
["REIKU-G","VMAVG-12M16"]
["REIKU-G","VMAVG-12M20"]
["REIKU-G","VMAVG-12P11"]
["REIKU-G","VMAVG-17M20"]
["REIKU-G","VMAVG-17M25"]
["REIKU-G","VMAVG-17P13"]
["REIKU-G","VMAVG-17P16"]
["REIKU-G","VMAVG-23M32"]
["REIKU-G","VMAVG-23P21"]
["REIKU-G","VMAVG-29M40"]
["REIKU-G","VMAVG-29P29"]
["REIKU-G","VMAVG-36M40"]
["REIKU-G","VMAVG-36M50"]
["REIKU-G","VMAVG-36P36"]
["REIKU-G","VMAVG-48M63"]
["REIKU-G","VMAVG-48P48"]
["REIKU-B","VMBRB-10M16"]
["REIKU-B","VMBRB-10M20"]
["REIKU-B","VMBRB-10P09"]
["REIKU-B","VMBRB-10P11"]
["REIKU-B","VMBRB-10P13"]
["REIKU-B","VMBRB-12M16"]
["REIKU-B","VMBRB-12M20"]
["REIKU-B","VMBRB-12P11"]
["REIKU-B","VMBRB-12P13"]
["REIKU-B","VMBRB-17M20"]
["REIKU-B","VMBRB-17M25"]
["REIKU-B","VMBRB-17P13"]
["REIKU-B","VMBRB-17P16"]
["REIKU-B","VMBRB-23M32"]
["REIKU-B","VMBRB-23P21"]
["REIKU-B","VMBRB-29M32"]
["REIKU-B","VMBRB-29M40"]
["REIKU-B","VMBRB-29P29"]
["REIKU-B","VMBRB-36M40"]
["REIKU-B","VMBRB-36M50"]
["REIKU-B","VMBRB-36P36"]
["REIKU-B","VMBRB-48M63"]
["REIKU-B","VMBRB-48P48"]
["REIKU-G","VMBRG-10M16"]
["REIKU-G","VMBRG-10M20"]
["REIKU-G","VMBRG-10P09"]
["REIKU-G","VMBRG-10P11"]
["REIKU-G","VMBRG-10P13"]
["REIKU-G","VMBRG-12M16"]
["REIKU-G","VMBRG-12M20"]
["REIKU-G","VMBRG-12P11"]
["REIKU-G","VMBRG-12P13"]
["REIKU-G","VMBRG-17M20"]
["REIKU-G","VMBRG-17M25"]
["REIKU-G","VMBRG-17P13"]
["REIKU-G","VMBRG-17P16"]
["REIKU-G","VMBRG-23M32"]
["REIKU-G","VMBRG-23P21"]
["REIKU-G","VMBRG-29M32"]
["REIKU-G","VMBRG-29M40"]
["REIKU-G","VMBRG-29P29"]
["REIKU-G","VMBRG-36M40"]
["REIKU-G","VMBRG-36M50"]
["REIKU-G","VMBRG-36P36"]
["REIKU-G","VMBRG-48M63"]
["REIKU-G","VMBRG-48P48"]
["REIKU-B","VMBVB-10M16"]
["REIKU-B","VMBVB-10M20"]
["REIKU-B","VMBVB-10P09"]
["REIKU-B","VMBVB-10P11"]
["REIKU-B","VMBVB-10P13"]
["REIKU-B","VMBVB-12M16"]
["REIKU-B","VMBVB-12M20"]
["REIKU-B","VMBVB-12P11"]
["REIKU-B","VMBVB-12P13"]
["REIKU-B","VMBVB-17M20"]
["REIKU-B","VMBVB-17M25"]
["REIKU-B","VMBVB-17P13"]
["REIKU-B","VMBVB-17P16"]
["REIKU-B","VMBVB-23M32"]
["REIKU-B","VMBVB-23P21"]
["REIKU-B","VMBVB-29M40"]
["REIKU-B","VMBVB-29P29"]
["REIKU-B","VMBVB-36M40"]
["REIKU-B","VMBVB-36M50"]
["REIKU-B","VMBVB-36P36"]
["REIKU-B","VMBVB-48M63"]
["REIKU-B","VMBVB-48P48"]
["REIKU-G","VMBVG-10M16"]
["REIKU-G","VMBVG-10M20"]
["REIKU-G","VMBVG-10P09"]
["REIKU-G","VMBVG-10P11"]
["REIKU-G","VMBVG-10P13"]
["REIKU-G","VMBVG-12M16"]
["REIKU-G","VMBVG-12M20"]
["REIKU-G","VMBVG-12P11"]
["REIKU-G","VMBVG-12P13"]
["REIKU-G","VMBVG-17M20"]
["REIKU-G","VMBVG-17M25"]
["REIKU-G","VMBVG-17P13"]
["REIKU-G","VMBVG-17P16"]
["REIKU-G","VMBVG-23M32"]
["REIKU-G","VMBVG-23P21"]
["REIKU-G","VMBVG-29M32"]
["REIKU-G","VMBVG-29M40"]
["REIKU-G","VMBVG-29P29"]
["REIKU-G","VMBVG-36M40"]
["REIKU-G","VMBVG-36M50"]
["REIKU-G","VMBVG-36P36"]
["REIKU-G","VMBVG-48M63"]
["REIKU-G","VMBVG-48P48"]
["REIKU-B","VMEVB-10M16"]
["REIKU-B","VMEVB-12M20"]
["REIKU-B","VMEVB-17M20"]
["REIKU-B","VMEVB-17M25"]
["REIKU-B","VMEVB-23M32"]
["REIKU-B","VMEVB-29M40"]
["REIKU-B","VMEVB-36M50"]
["REIKU-B","VMEVB-48M50"]
["REIKU-B","VMGRB-10M16"]
["REIKU-B","VMGRB-10M20"]
["REIKU-B","VMGRB-10P09"]
["REIKU-B","VMGRB-12M16"]
["REIKU-B","VMGRB-12M20"]
["REIKU-B","VMGRB-12P11"]
["REIKU-B","VMGRB-17M20"]
["REIKU-B","VMGRB-17M25"]
["REIKU-B","VMGRB-17P13"]
["REIKU-B","VMGRB-17P16"]
["REIKU-B","VMGRB-23M25"]
["REIKU-B","VMGRB-23M32"]
["REIKU-B","VMGRB-23P21"]
["REIKU-B","VMGRB-29M32"]
["REIKU-B","VMGRB-29M40"]
["REIKU-B","VMGRB-29P29"]
["REIKU-B","VMGRB-36M40"]
["REIKU-B","VMGRB-36M50"]
["REIKU-B","VMGRB-36P36"]
["REIKU-B","VMGRB-48M63"]
["REIKU-B","VMGRB-48P48"]
["REIKU-G","VMGRG-10M16"]
["REIKU-G","VMGRG-10M20"]
["REIKU-G","VMGRG-10P09"]
["REIKU-G","VMGRG-12M16"]
["REIKU-G","VMGRG-12M20"]
["REIKU-G","VMGRG-12P11"]
["REIKU-G","VMGRG-17M20"]
["REIKU-G","VMGRG-17M25"]
["REIKU-G","VMGRG-17P13"]
["REIKU-G","VMGRG-17P16"]
["REIKU-G","VMGRG-23M25"]
["REIKU-G","VMGRG-23M32"]
["REIKU-G","VMGRG-23P21"]
["REIKU-G","VMGRG-29M32"]
["REIKU-G","VMGRG-29M40"]
["REIKU-G","VMGRG-29P29"]
["REIKU-G","VMGRG-36M40"]
["REIKU-G","VMGRG-36M50"]
["REIKU-G","VMGRG-36P36"]
["REIKU-G","VMGRG-48M63"]
["REIKU-G","VMGRG-48P48"]
["REIKU-B","VMGVB-10M16"]
["REIKU-B","VMGVB-10M16Z"]
["REIKU-B","VMGVB-10M20"]
["REIKU-B","VMGVB-10P09"]
["REIKU-B","VMGVB-12M16"]
["REIKU-B","VMGVB-12M16Z"]
["REIKU-B","VMGVB-12M20"]
["REIKU-B","VMGVB-12M20Z"]
["REIKU-B","VMGVB-12P11"]
["REIKU-B","VMGVB-17M20"]
["REIKU-B","VMGVB-17M20Z"]
["REIKU-B","VMGVB-17M25"]
["REIKU-B","VMGVB-17P13"]
["REIKU-B","VMGVB-17P16"]
["REIKU-B","VMGVB-23M25"]
["REIKU-B","VMGVB-23M25Z"]
["REIKU-B","VMGVB-23M32"]
["REIKU-B","VMGVB-23P21"]
["REIKU-B","VMGVB-29M32"]
["REIKU-B","VMGVB-29M32Z"]
["REIKU-B","VMGVB-29M40"]
["REIKU-B","VMGVB-29P29"]
["REIKU-B","VMGVB-36M40"]
["REIKU-B","VMGVB-36M40Z"]
["REIKU-B","VMGVB-36M50"]
["REIKU-B","VMGVB-36P36"]
["REIKU-B","VMGVB-48M63"]
["REIKU-B","VMGVB-48M63Z"]
["REIKU-B","VMGVB-48P48"]
["REIKU-G","VMGVG-10M16"]
["REIKU-G","VMGVG-10M16Z"]
["REIKU-G","VMGVG-10M20"]
["REIKU-G","VMGVG-10P09"]
["REIKU-G","VMGVG-12M16"]
["REIKU-G","VMGVG-12M16Z"]
["REIKU-G","VMGVG-12M20"]
["REIKU-G","VMGVG-12M20Z"]
["REIKU-G","VMGVG-12P11"]
["REIKU-G","VMGVG-17M20"]
["REIKU-G","VMGVG-17M20Z"]
["REIKU-G","VMGVG-17M25"]
["REIKU-G","VMGVG-17P13"]
["REIKU-G","VMGVG-17P16"]
["REIKU-G","VMGVG-23M25"]
["REIKU-G","VMGVG-23M25Z"]
["REIKU-G","VMGVG-23M32"]
["REIKU-G","VMGVG-23P21"]
["REIKU-G","VMGVG-29M32"]
["REIKU-G","VMGVG-29M32Z"]
["REIKU-G","VMGVG-29M40"]
["REIKU-G","VMGVG-29P29"]
["REIKU-G","VMGVG-36M40"]
["REIKU-G","VMGVG-36M40Z"]
["REIKU-G","VMGVG-36M50"]
["REIKU-G","VMGVG-36P36"]
["REIKU-G","VMGVG-48M63"]
["REIKU-G","VMGVG-48M63Z"]
["REIKU-G","VMGVG-48P48"]
["REIKU-B","VMIRB-17M25"]
["REIKU-B","VMIRB-23M25"]
["REIKU-B","VMIRB-29M40"]
["REIKU-B","VMIRB-36M50"]
["REIKU-B","VMSVB-12/18"]
["REIKU-B","VMSVB-17/20"]
["REIKU-B","VMSVB-17/22"]
["REIKU-B","VMSVB-17/25"]
["REIKU-B","VMSVB-23/28"]
["REIKU-B","VMSVB-29/32"]
["REIKU-B","VMSVB-29/37"]
["REIKU-B","VMSVB-36/40"]
["REIKU-B","VMSVB-36/47"]
["REIKU-B","VMSVB-48/59"]
["REIKU-G","VMSVG-12/18"]
["REIKU-G","VMSVG-17/20"]
["REIKU-G","VMSVG-17/22"]
["REIKU-G","VMSVG-17/25"]
["REIKU-G","VMSVG-23/28"]
["REIKU-G","VMSVG-29/32"]
["REIKU-G","VMSVG-29/37"]
["REIKU-G","VMSVG-36/40"]
["REIKU-G","VMSVG-36/47"]
["REIKU-G","VMSVG-48/59"]
["TECHNIK","VN  0,5-M 2"]
["TECHNIK","VN  0,5-M 3"]
["TECHNIK","VN  0,5-M 3,5"]
["TECHNIK","VN  0,5-M 4"]
["TECHNIK","VN  0,5-M 5"]
["TECHNIK","VN  1,5-M 3"]
["TECHNIK","VN  1,5-M 3,5"]
["TECHNIK","VN  1,5-M 3,5/7"]
["TECHNIK","VN  1,5-M 4"]
["TECHNIK","VN  1,5-M 4/7"]
["TECHNIK","VN  1,5-M 5"]
["TECHNIK","VN  1,5-M 5/10"]
["TECHNIK","VN  1,5-M 6"]
["TECHNIK","VN  1,5-M 6/9"]
["TECHNIK","VN  1,5-M 8"]
["TECHNIK","VN  1,5-M10"]
["TECHNIK","VN  1,5-M12"]
["TECHNIK","VN  2,5-M 3"]
["TECHNIK","VN  2,5-M 3,5"]
["TECHNIK","VN  2,5-M 4"]
["TECHNIK","VN  2,5-M 4/7"]
["TECHNIK","VN  2,5-M 5"]
["TECHNIK","VN  2,5-M 6"]
["TECHNIK","VN  2,5-M 8"]
["TECHNIK","VN  2,5-M10"]
["TECHNIK","VN  2,5-M12"]
["TECHNIK","VN  6-M 3,5"]
["TECHNIK","VN  6-M 4"]
["TECHNIK","VN  6-M 5"]
["TECHNIK","VN  6-M 6"]
["TECHNIK","VN  6-M 8"]
["TECHNIK","VN  6-M10"]
["TECHNIK","VN  6-M12"]
["TECHNIK","VN  6-M16"]
["TECHNIK","VN 10-M 4"]
["TECHNIK","VN 10-M 5"]
["TECHNIK","VN 10-M 6"]
["TECHNIK","VN 10-M 8"]
["TECHNIK","VN 10-M10"]
["TECHNIK","VN 16-M 5"]
["TECHNIK","VN 16-M 6"]
["TECHNIK","VN 16-M 8"]
["TECHNIK","VN 16-M10"]
["TECHNIK","VNN  1,5-M4"]
["TECHNIK","VNN  1,5-M5"]
["TECHNIK","VNN  2,5-M4"]
["TECHNIK","VNN  2,5-M5"]
["TECHNIK","VNN  6-M5"]
["TECHNIK","VP 2,5x100 fialová"]
["TECHNIK","VP 2,5x100 hnědá"]
["TECHNIK","VP 2,5x100 modrá"]
["TECHNIK","VP 2,5x100 oranžová"]
["TECHNIK","VP 2,5x100 rudá"]
["TECHNIK","VP 2,5x100 šedá"]
["TECHNIK","VP 2,5x100 zelená"]
["TECHNIK","VP 2,5x100 žlutá"]
["TECHNIK","VP 2,5x200 fialová"]
["TECHNIK","VP 2,5x200 hnědá"]
["TECHNIK","VP 2,5x200 modrá"]
["TECHNIK","VP 2,5x200 oranžová"]
["TECHNIK","VP 2,5x200 rudá"]
["TECHNIK","VP 2,5x200 šedá"]
["TECHNIK","VP 2,5x200 zelená"]
["TECHNIK","VP 2,5x200 žlutá"]
["TECHNIK","VP 3,6x140 hnědá"]
["TECHNIK","VP 3,6x140 modrá"]
["TECHNIK","VP 3,6x140 oranžová"]
["TECHNIK","VP 3,6x140 rudá"]
["TECHNIK","VP 3,6x140 šedá"]
["TECHNIK","VP 3,6x140 zelená"]
["TECHNIK","VP 3,6x140 zelená UV"]
["TECHNIK","VP 3,6x140 žlutá"]
["TECHNIK","VP 3,6x200 fialová"]
["TECHNIK","VP 3,6x200 modrá"]
["TECHNIK","VP 3,6x200 oranžová"]
["TECHNIK","VP 3,6x200 rudá"]
["TECHNIK","VP 3,6x200 šedá"]
["TECHNIK","VP 3,6x200 zelená"]
["TECHNIK","VP 3,6x200 žlutá"]
["TECHNIK","VP 3,6x300 modrá"]
["TECHNIK","VP 3,6x300 rudá"]
["TECHNIK","VP 3,6x300 zelená"]
["TECHNIK","VP 3,6x300 žlutá"]
["TECHNIK","VP 4,8x200 fialová"]
["TECHNIK","VP 4,8x200 hnědá"]
["TECHNIK","VP 4,8x200 modrá"]
["TECHNIK","VP 4,8x200 oranžová"]
["TECHNIK","VP 4,8x200 rudá"]
["TECHNIK","VP 4,8x200 šedá"]
["TECHNIK","VP 4,8x200 zelená"]
["TECHNIK","VP 4,8x200 zelená UV"]
["TECHNIK","VP 4,8x200 žlutá"]
["TECHNIK","VP 4,8x250 fialová"]
["TECHNIK","VP 4,8x250 modrá"]
["TECHNIK","VP 4,8x250 rudá"]
["TECHNIK","VP 4,8x250 šedá"]
["TECHNIK","VP 4,8x250 zelená"]
["TECHNIK","VP 4,8x250 žlutá"]
["TECHNIK","VP 4,8x300 fialová"]
["TECHNIK","VP 4,8x300 hnědá"]
["TECHNIK","VP 4,8x300 modrá"]
["TECHNIK","VP 4,8x300 oranžová"]
["TECHNIK","VP 4,8x300 rudá"]
["TECHNIK","VP 4,8x300 šedá"]
["TECHNIK","VP 4,8x300 zelená"]
["TECHNIK","VP 4,8x300 žlutá"]
["TECHNIK","VP 4,8x370 hnědá"]
["TECHNIK","VP 4,8x370 modrá"]
["TECHNIK","VP 4,8x370 rudá"]
["TECHNIK","VP 4,8x370 zelená"]
["TECHNIK","VP 4,8x370 žlutá"]
["TECHNIK","VP 7,6x250 zelená UV"]
["TECHNIK","VP 7,6x370 modrá"]
["TECHNIK","VP 7,6x370 rudá"]
["TECHNIK","VP 7,6x370 zelená"]
["TECHNIK","VP 7,6x370 žlutá"]
["TECHNIK","VP 9,0x530 zelená"]
["TECHNIK","VP 9,0x780 šedá"]
["TECHNIK","VP CLIP 4,8x150"]
["REIKU-B","VP connector NW 07"]
["REIKU-B","VP connector NW 10"]
["REIKU-B","VP connector NW 12"]
["REIKU-B","VP connector NW 17"]
["TECHNIK","VP RAPSTRAP černá"]
["TECHNIK","VP RAPSTRAP přírodní"]
["TECHNIK","VP RAPSTRAP rudá"]
["TECHNIK","VP RAPSTRAP zelená"]
["REIKU-B","VPARB-10G01"]
["REIKU-B","VPARB-10M16"]
["REIKU-B","VPARB-10M20"]
["REIKU-B","VPARB-10P09"]
["REIKU-B","VPARB-12G01"]
["REIKU-B","VPARB-12M16"]
["REIKU-B","VPARB-12M20"]
["REIKU-B","VPARB-12P11"]
["REIKU-B","VPARB-17G02"]
["REIKU-B","VPARB-17M20"]
["REIKU-B","VPARB-17M25"]
["REIKU-B","VPARB-17P16"]
["REIKU-B","VPARB-23G03"]
["REIKU-B","VPARB-23M25"]
["REIKU-B","VPARB-23M32"]
["REIKU-B","VPARB-23P21"]
["REIKU-B","VPARB-29G04"]
["REIKU-B","VPARB-29M32"]
["REIKU-B","VPARB-29M40"]
["REIKU-B","VPARB-29P29"]
["REIKU-B","VPARB-36G05"]
["REIKU-B","VPARB-36M40"]
["REIKU-B","VPARB-36M50"]
["REIKU-B","VPARB-36P36"]
["REIKU-B","VPARB-48G07"]
["REIKU-B","VPARB-48M50"]
["REIKU-B","VPARB-48M63"]
["REIKU-B","VPARB-48P48"]
["REIKU-G","VPARG-10G01"]
["REIKU-G","VPARG-10M16"]
["REIKU-G","VPARG-10M20"]
["REIKU-G","VPARG-10P09"]
["REIKU-G","VPARG-12G01"]
["REIKU-G","VPARG-12M16"]
["REIKU-G","VPARG-12M20"]
["REIKU-G","VPARG-12P11"]
["REIKU-G","VPARG-17G02"]
["REIKU-G","VPARG-17M20"]
["REIKU-G","VPARG-17M25"]
["REIKU-G","VPARG-17P16"]
["REIKU-G","VPARG-23G03"]
["REIKU-G","VPARG-23M25"]
["REIKU-G","VPARG-23M32"]
["REIKU-G","VPARG-23P21"]
["REIKU-G","VPARG-29G04"]
["REIKU-G","VPARG-29M32"]
["REIKU-G","VPARG-29M40"]
["REIKU-G","VPARG-29P29"]
["REIKU-G","VPARG-36G05"]
["REIKU-G","VPARG-36M40"]
["REIKU-G","VPARG-36M50"]
["REIKU-G","VPARG-36P36"]
["REIKU-G","VPARG-48G07"]
["REIKU-G","VPARG-48M50"]
["REIKU-G","VPARG-48M63"]
["REIKU-G","VPARG-48P48"]
["REIKU-B","VPAVB-10M16"]
["REIKU-B","VPAVB-10M20"]
["REIKU-B","VPAVB-10P09"]
["REIKU-B","VPAVB-12M16"]
["REIKU-B","VPAVB-12M20"]
["REIKU-B","VPAVB-12P11"]
["REIKU-B","VPAVB-17M20"]
["REIKU-B","VPAVB-17M25"]
["REIKU-B","VPAVB-17P16"]
["REIKU-B","VPAVB-23M25"]
["REIKU-B","VPAVB-23M32"]
["REIKU-B","VPAVB-23P21"]
["REIKU-B","VPAVB-29M32"]
["REIKU-B","VPAVB-29M40"]
["REIKU-B","VPAVB-29P29"]
["REIKU-B","VPAVB-36M40"]
["REIKU-B","VPAVB-36M50"]
["REIKU-B","VPAVB-36P36"]
["REIKU-B","VPAVB-48M50"]
["REIKU-B","VPAVB-48M63"]
["REIKU-B","VPAVB-48P48"]
["REIKU-G","VPAVG-10M16"]
["REIKU-G","VPAVG-10M20"]
["REIKU-G","VPAVG-10P09"]
["REIKU-G","VPAVG-12M16"]
["REIKU-G","VPAVG-12M20"]
["REIKU-G","VPAVG-12P11"]
["REIKU-G","VPAVG-17M20"]
["REIKU-G","VPAVG-17M25"]
["REIKU-G","VPAVG-17P16"]
["REIKU-G","VPAVG-23M25"]
["REIKU-G","VPAVG-23M32"]
["REIKU-G","VPAVG-23P21"]
["REIKU-G","VPAVG-29M32"]
["REIKU-G","VPAVG-29M40"]
["REIKU-G","VPAVG-29P29"]
["REIKU-G","VPAVG-36M40"]
["REIKU-G","VPAVG-36M50"]
["REIKU-G","VPAVG-36P36"]
["REIKU-G","VPAVG-48M50"]
["REIKU-G","VPAVG-48M63"]
["REIKU-G","VPAVG-48P48"]
["REIKU-B","VPBRB-10G01"]
["REIKU-B","VPBRB-10M16"]
["REIKU-B","VPBRB-10M20"]
["REIKU-B","VPBRB-10P09"]
["REIKU-B","VPBRB-10P11"]
["REIKU-B","VPBRB-10P13"]
["REIKU-B","VPBRB-12G01"]
["REIKU-B","VPBRB-12M16"]
["REIKU-B","VPBRB-12M20"]
["REIKU-B","VPBRB-12P11"]
["REIKU-B","VPBRB-12P13"]
["REIKU-B","VPBRB-17G02"]
["REIKU-B","VPBRB-17M20"]
["REIKU-B","VPBRB-17M25"]
["REIKU-B","VPBRB-17P13"]
["REIKU-B","VPBRB-17P16"]
["REIKU-B","VPBRB-23G03"]
["REIKU-B","VPBRB-23M25"]
["REIKU-B","VPBRB-23M32"]
["REIKU-B","VPBRB-23P21"]
["REIKU-B","VPBRB-29G04"]
["REIKU-B","VPBRB-29M32"]
["REIKU-B","VPBRB-29M40"]
["REIKU-B","VPBRB-29P29"]
["REIKU-B","VPBRB-36G05"]
["REIKU-B","VPBRB-36M40"]
["REIKU-B","VPBRB-36M50"]
["REIKU-B","VPBRB-36P36"]
["REIKU-B","VPBRB-48G07"]
["REIKU-B","VPBRB-48M50"]
["REIKU-B","VPBRB-48M63"]
["REIKU-B","VPBRB-48P48"]
["REIKU-G","VPBRG-10G01"]
["REIKU-G","VPBRG-10M16"]
["REIKU-G","VPBRG-10M20"]
["REIKU-G","VPBRG-10P09"]
["REIKU-G","VPBRG-10P11"]
["REIKU-G","VPBRG-10P13"]
["REIKU-G","VPBRG-12G01"]
["REIKU-G","VPBRG-12M16"]
["REIKU-G","VPBRG-12M20"]
["REIKU-G","VPBRG-12P11"]
["REIKU-G","VPBRG-12P13"]
["REIKU-G","VPBRG-17G02"]
["REIKU-G","VPBRG-17M20"]
["REIKU-G","VPBRG-17M25"]
["REIKU-G","VPBRG-17P13"]
["REIKU-G","VPBRG-17P16"]
["REIKU-G","VPBRG-23G03"]
["REIKU-G","VPBRG-23M25"]
["REIKU-G","VPBRG-23M32"]
["REIKU-G","VPBRG-23P21"]
["REIKU-G","VPBRG-29G04"]
["REIKU-G","VPBRG-29M32"]
["REIKU-G","VPBRG-29M40"]
["REIKU-G","VPBRG-29P29"]
["REIKU-G","VPBRG-36G05"]
["REIKU-G","VPBRG-36M40"]
["REIKU-G","VPBRG-36M50"]
["REIKU-G","VPBRG-36P36"]
["REIKU-G","VPBRG-48G07"]
["REIKU-G","VPBRG-48M50"]
["REIKU-G","VPBRG-48M63"]
["REIKU-G","VPBRG-48P48"]
["REIKU-B","VPBVB-10M16"]
["REIKU-B","VPBVB-10M20"]
["REIKU-B","VPBVB-10P09"]
["REIKU-B","VPBVB-10P11"]
["REIKU-B","VPBVB-10P13"]
["REIKU-B","VPBVB-12M16"]
["REIKU-B","VPBVB-12M20"]
["REIKU-B","VPBVB-12P11"]
["REIKU-B","VPBVB-12P13"]
["REIKU-B","VPBVB-17M20"]
["REIKU-B","VPBVB-17M25"]
["REIKU-B","VPBVB-17P13"]
["REIKU-B","VPBVB-17P16"]
["REIKU-B","VPBVB-23M25"]
["REIKU-B","VPBVB-23M32"]
["REIKU-B","VPBVB-23P21"]
["REIKU-B","VPBVB-29M32"]
["REIKU-B","VPBVB-29M40"]
["REIKU-B","VPBVB-29P29"]
["REIKU-B","VPBVB-36M40"]
["REIKU-B","VPBVB-36M50"]
["REIKU-B","VPBVB-36P36"]
["REIKU-B","VPBVB-48M50"]
["REIKU-B","VPBVB-48M63"]
["REIKU-B","VPBVB-48P48"]
["REIKU-G","VPBVG-10M16"]
["REIKU-G","VPBVG-10M20"]
["REIKU-G","VPBVG-10P09"]
["REIKU-G","VPBVG-10P11"]
["REIKU-G","VPBVG-10P13"]
["REIKU-G","VPBVG-12M16"]
["REIKU-G","VPBVG-12M20"]
["REIKU-G","VPBVG-12P11"]
["REIKU-G","VPBVG-12P13"]
["REIKU-G","VPBVG-17M20"]
["REIKU-G","VPBVG-17M25"]
["REIKU-G","VPBVG-17P13"]
["REIKU-G","VPBVG-17P16"]
["REIKU-G","VPBVG-23M25"]
["REIKU-G","VPBVG-23M32"]
["REIKU-G","VPBVG-23P21"]
["REIKU-G","VPBVG-29M32"]
["REIKU-G","VPBVG-29M40"]
["REIKU-G","VPBVG-29P29"]
["REIKU-G","VPBVG-36M40"]
["REIKU-G","VPBVG-36M50"]
["REIKU-G","VPBVG-36P36"]
["REIKU-G","VPBVG-48M50"]
["REIKU-G","VPBVG-48M63"]
["REIKU-G","VPBVG-48P48"]
["TECHNIK","VPC  1,7x70"]
["TECHNIK","VPC  1,9x100"]
["TECHNIK","VPC  2,4x60"]
["TECHNIK","VPC  2,4x80"]
["TECHNIK","VPC  2,5x100"]
["TECHNIK","VPC  2,5x100 UV"]
["TECHNIK","VPC  2,5x100/1000"]
["TECHNIK","VPC  2,5x120"]
["TECHNIK","VPC  2,5x140"]
["TECHNIK","VPC  2,5x160"]
["TECHNIK","VPC  2,5x200"]
["TECHNIK","VPC  2,5x200/1000"]
["TECHNIK","VPC  3,6x140"]
["TECHNIK","VPC  3,6x140 UV"]
["TECHNIK","VPC  3,6x140/1000"]
["TECHNIK","VPC  3,6x150"]
["TECHNIK","VPC  3,6x180"]
["TECHNIK","VPC  3,6x200"]
["TECHNIK","VPC  3,6x200 UV"]
["TECHNIK","VPC  3,6x250"]
["TECHNIK","VPC  3,6x300"]
["TECHNIK","VPC  3,6x370"]
["TECHNIK","VPC  4,8x120"]
["TECHNIK","VPC  4,8x160"]
["TECHNIK","VPC  4,8x188"]
["TECHNIK","VPC  4,8x200"]
["TECHNIK","VPC  4,8x200 UV"]
["TECHNIK","VPC  4,8x200 Z"]
["TECHNIK","VPC  4,8x200/1000"]
["TECHNIK","VPC  4,8x250"]
["TECHNIK","VPC  4,8x280"]
["TECHNIK","VPC  4,8x300"]
["TECHNIK","VPC  4,8x300 UV"]
["TECHNIK","VPC  4,8x300/1000"]
["TECHNIK","VPC  4,8x370"]
["TECHNIK","VPC  4,8x385"]
["TECHNIK","VPC  4,8x430"]
["TECHNIK","VPC  4,8x530"]
["TECHNIK","VPC  4,8x680"]
["TECHNIK","VPC  4,8x830"]
["TECHNIK","VPC  7,6x150"]
["TECHNIK","VPC  7,6x200"]
["TECHNIK","VPC  7,6x240"]
["TECHNIK","VPC  7,6x300"]
["TECHNIK","VPC  7,6x370"]
["TECHNIK","VPC  7,6x370 UV"]
["TECHNIK","VPC  7,8x450"]
["TECHNIK","VPC  7,8x500"]
["TECHNIK","VPC  7,8x550"]
["TECHNIK","VPC  7,8x750"]
["TECHNIK","VPC  9,0x 430"]
["TECHNIK","VPC  9,0x 430 UV"]
["TECHNIK","VPC  9,0x 530"]
["TECHNIK","VPC  9,0x 760 D"]
["TECHNIK","VPC  9,0x 780"]
["TECHNIK","VPC  9,0x 920"]
["TECHNIK","VPC  9,0x1020"]
["TECHNIK","VPC  9,0x1220"]
["TECHNIK","VPC  9,0x1530"]
["TECHNIK","VPC 13x 230"]
["TECHNIK","VPC 13x 380"]
["TECHNIK","VPC 13x 480"]
["TECHNIK","VPC 13x 580"]
["TECHNIK","VPC 13x 730"]
["TECHNIK","VPC 13x 830"]
["TECHNIK","VPC 13x1000"]
["TECHNIK","VPC+ 2,5x100"]
["TECHNIK","VPC+ 2,5x160"]
["TECHNIK","VPC+ 2,5x200"]
["TECHNIK","VPC+ 3,6x140"]
["TECHNIK","VPC+ 3,6x200"]
["TECHNIK","VPC+ 3,6x250"]
["TECHNIK","VPC+ 3,6x370"]
["TECHNIK","VPC+ 4,8x200"]
["TECHNIK","VPC+ 4,8x300"]
["TECHNIK","VPC+ 4,8x370"]
["TECHNIK","VPC+ 4,8x430"]
["TECHNIK","VPC+ 4,8x530"]
["TECHNIK","VPC+ 7,6x370"]
["TECHNIK","VPC+ 9,0x780"]
["TECHNIK","VPCDO 2,5x110"]
["TECHNIK","VPCDO 3,6x150"]
["TECHNIK","VPCDO 4,8x190"]
["TECHNIK","VPCDO 4,8x200"]
["TECHNIK","VPCDO 4,8x201"]
["TECHNIK","VPCFE 2,4x 90"]
["TECHNIK","VPCFE 2,4x200"]
["TECHNIK","VPCFE 3,6x140"]
["TECHNIK","VPCFE 3,6x200"]
["TECHNIK","VPCFE 3,6x280"]
["TECHNIK","VPCFE 3,6x370"]
["TECHNIK","VPCFE 4,8x180"]
["TECHNIK","VPCFE 4,8x290"]
["TECHNIK","VPCFE 4,8x360"]
["TECHNIK","VPCFE 7,6x222"]
["TECHNIK","VPCFE 7,6x340"]
["TECHNIK","VPCFE 7,6x760"]
["TECHNIK","VPCRO 3,6x100"]
["TECHNIK","VPCRO 4,8x150"]
["TECHNIK","VPCRO 4,8x200"]
["TECHNIK","VPCRO 4,8x250"]
["TECHNIK","VPCRO 4,8x300"]
["TECHNIK","VPCRO 4,8x370"]
["TECHNIK","VPCRO 7,6x120"]
["TECHNIK","VPCRO 7,6x150"]
["TECHNIK","VPCRO 7,6x200"]
["TECHNIK","VPCRO 7,6x250"]
["TECHNIK","VPCRO 7,6x300"]
["TECHNIK","VPCRO12,4x400"]
["TECHNIK","VPCRO12,4x500"]
["TECHNIK","VPDO 2,5x110"]
["TECHNIK","VPDO 3,6x150"]
["TECHNIK","VPDO 4,8x130"]
["TECHNIK","VPDO 4,8x200"]
["REIKU-B","VPGRB-10G00"]
["REIKU-B","VPGRB-10M12"]
["REIKU-B","VPGRB-10M16"]
["REIKU-B","VPGRB-10M16Z"]
["REIKU-B","VPGRB-10M20"]
["REIKU-B","VPGRB-10P07"]
["REIKU-B","VPGRB-10P09"]
["REIKU-B","VPGRB-10P11"]
["REIKU-B","VPGRB-10P13"]
["REIKU-B","VPGRB-12G01"]
["REIKU-B","VPGRB-12G02"]
["REIKU-B","VPGRB-12M16"]
["REIKU-B","VPGRB-12M16Z"]
["REIKU-B","VPGRB-12M20"]
["REIKU-B","VPGRB-12M20Z"]
["REIKU-B","VPGRB-12P09"]
["REIKU-B","VPGRB-12P11"]
["REIKU-B","VPGRB-12P13"]
["REIKU-B","VPGRB-17G02"]
["REIKU-B","VPGRB-17M20"]
["REIKU-B","VPGRB-17M20Z"]
["REIKU-B","VPGRB-17M25"]
["REIKU-B","VPGRB-17M32"]
["REIKU-B","VPGRB-17P11"]
["REIKU-B","VPGRB-17P13"]
["REIKU-B","VPGRB-17P16"]
["REIKU-B","VPGRB-17P21"]
["REIKU-B","VPGRB-23G03"]
["REIKU-B","VPGRB-23M25"]
["REIKU-B","VPGRB-23M25Z"]
["REIKU-B","VPGRB-23M32"]
["REIKU-B","VPGRB-23P16"]
["REIKU-B","VPGRB-23P21"]
["REIKU-B","VPGRB-29G04"]
["REIKU-B","VPGRB-29M32"]
["REIKU-B","VPGRB-29M32Z"]
["REIKU-B","VPGRB-29M40"]
["REIKU-B","VPGRB-29P29"]
["REIKU-B","VPGRB-36G05"]
["REIKU-B","VPGRB-36M40"]
["REIKU-B","VPGRB-36M40Z"]
["REIKU-B","VPGRB-36M50"]
["REIKU-B","VPGRB-36P29"]
["REIKU-B","VPGRB-36P36"]
["REIKU-B","VPGRB-48G06"]
["REIKU-B","VPGRB-48G07"]
["REIKU-B","VPGRB-48M50"]
["REIKU-B","VPGRB-48M63"]
["REIKU-B","VPGRB-48M63Z"]
["REIKU-B","VPGRB-48P42"]
["REIKU-B","VPGRB-48P48"]
["REIKU-G","VPGRG-10G00"]
["REIKU-G","VPGRG-10M12"]
["REIKU-G","VPGRG-10M16"]
["REIKU-G","VPGRG-10M16Z"]
["REIKU-G","VPGRG-10M20"]
["REIKU-G","VPGRG-10P07"]
["REIKU-G","VPGRG-10P09"]
["REIKU-G","VPGRG-10P11"]
["REIKU-G","VPGRG-10P13"]
["REIKU-G","VPGRG-12G01"]
["REIKU-G","VPGRG-12G02"]
["REIKU-G","VPGRG-12M16"]
["REIKU-G","VPGRG-12M16Z"]
["REIKU-G","VPGRG-12M20"]
["REIKU-G","VPGRG-12M20Z"]
["REIKU-G","VPGRG-12P09"]
["REIKU-G","VPGRG-12P11"]
["REIKU-G","VPGRG-12P13"]
["REIKU-G","VPGRG-17G02"]
["REIKU-G","VPGRG-17M20"]
["REIKU-G","VPGRG-17M20Z"]
["REIKU-G","VPGRG-17M25"]
["REIKU-G","VPGRG-17M32"]
["REIKU-G","VPGRG-17P11"]
["REIKU-G","VPGRG-17P13"]
["REIKU-G","VPGRG-17P16"]
["REIKU-G","VPGRG-17P21"]
["REIKU-G","VPGRG-23G03"]
["REIKU-G","VPGRG-23M25"]
["REIKU-G","VPGRG-23M25Z"]
["REIKU-G","VPGRG-23M32"]
["REIKU-G","VPGRG-23P16"]
["REIKU-G","VPGRG-23P21"]
["REIKU-G","VPGRG-29G04"]
["REIKU-G","VPGRG-29M32"]
["REIKU-G","VPGRG-29M32Z"]
["REIKU-G","VPGRG-29M40"]
["REIKU-G","VPGRG-29P29"]
["REIKU-G","VPGRG-36G05"]
["REIKU-G","VPGRG-36M40"]
["REIKU-G","VPGRG-36M40Z"]
["REIKU-G","VPGRG-36M50"]
["REIKU-G","VPGRG-36P29"]
["REIKU-G","VPGRG-36P36"]
["REIKU-G","VPGRG-48G06"]
["REIKU-G","VPGRG-48G07"]
["REIKU-G","VPGRG-48M50"]
["REIKU-G","VPGRG-48M63"]
["REIKU-G","VPGRG-48M63Z"]
["REIKU-G","VPGRG-48P42"]
["REIKU-G","VPGRG-48P48"]
["REIKU-B","VPGVB-10M12"]
["REIKU-B","VPGVB-10M16"]
["REIKU-B","VPGVB-10M20"]
["REIKU-B","VPGVB-10P07"]
["REIKU-B","VPGVB-10P09"]
["REIKU-B","VPGVB-10P11"]
["REIKU-B","VPGVB-10P13"]
["REIKU-B","VPGVB-10S15"]
["REIKU-B","VPGVB-12M16"]
["REIKU-B","VPGVB-12M20"]
["REIKU-B","VPGVB-12P09"]
["REIKU-B","VPGVB-12P11"]
["REIKU-B","VPGVB-12P13"]
["REIKU-B","VPGVB-12S19"]
["REIKU-B","VPGVB-17M20"]
["REIKU-B","VPGVB-17M25"]
["REIKU-B","VPGVB-17M32"]
["REIKU-B","VPGVB-17P11"]
["REIKU-B","VPGVB-17P13"]
["REIKU-B","VPGVB-17P16"]
["REIKU-B","VPGVB-17P21"]
["REIKU-B","VPGVB-17S22"]
["REIKU-B","VPGVB-23M25"]
["REIKU-B","VPGVB-23M32"]
["REIKU-B","VPGVB-23P16"]
["REIKU-B","VPGVB-23P21"]
["REIKU-B","VPGVB-23S28"]
["REIKU-B","VPGVB-23S32"]
["REIKU-B","VPGVB-29M32"]
["REIKU-B","VPGVB-29M40"]
["REIKU-B","VPGVB-29P29"]
["REIKU-B","VPGVB-29S37"]
["REIKU-B","VPGVB-29S40"]
["REIKU-B","VPGVB-36M40"]
["REIKU-B","VPGVB-36M50"]
["REIKU-B","VPGVB-36P29"]
["REIKU-B","VPGVB-36P36"]
["REIKU-B","VPGVB-48M50"]
["REIKU-B","VPGVB-48M63"]
["REIKU-B","VPGVB-48P42"]
["REIKU-B","VPGVB-48P48"]
["REIKU-G","VPGVG-10M12"]
["REIKU-G","VPGVG-10M16"]
["REIKU-G","VPGVG-10M20"]
["REIKU-G","VPGVG-10P07"]
["REIKU-G","VPGVG-10P09"]
["REIKU-G","VPGVG-10P11"]
["REIKU-G","VPGVG-10P13"]
["REIKU-G","VPGVG-10S15"]
["REIKU-G","VPGVG-12M16"]
["REIKU-G","VPGVG-12M20"]
["REIKU-G","VPGVG-12P09"]
["REIKU-G","VPGVG-12P11"]
["REIKU-G","VPGVG-12P13"]
["REIKU-G","VPGVG-12S19"]
["REIKU-G","VPGVG-17M20"]
["REIKU-G","VPGVG-17M25"]
["REIKU-G","VPGVG-17M32"]
["REIKU-G","VPGVG-17P11"]
["REIKU-G","VPGVG-17P13"]
["REIKU-G","VPGVG-17P16"]
["REIKU-G","VPGVG-17P21"]
["REIKU-G","VPGVG-17S22"]
["REIKU-G","VPGVG-23M25"]
["REIKU-G","VPGVG-23M32"]
["REIKU-G","VPGVG-23P16"]
["REIKU-G","VPGVG-23P21"]
["REIKU-G","VPGVG-23S28"]
["REIKU-G","VPGVG-23S32"]
["REIKU-G","VPGVG-29M32"]
["REIKU-G","VPGVG-29M40"]
["REIKU-G","VPGVG-29P29"]
["REIKU-G","VPGVG-29S37"]
["REIKU-G","VPGVG-29S40"]
["REIKU-G","VPGVG-36M40"]
["REIKU-G","VPGVG-36M50"]
["REIKU-G","VPGVG-36P29"]
["REIKU-G","VPGVG-36P36"]
["REIKU-G","VPGVG-48M50"]
["REIKU-G","VPGVG-48M63"]
["REIKU-G","VPGVG-48P42"]
["REIKU-G","VPGVG-48P48"]
["REIKU-B","VPHOB-12"]
["REIKU-B","VPHOB-17"]
["REIKU-B","VPHOB-23"]
["REIKU-B","VPHOB-29"]
["REIKU-B","VPHOB-36"]
["REIKU-B","VPHOB-42"]
["REIKU-B","VPHOB-48"]
["REIKU-B","VPIRB-10M121"]
["REIKU-B","VPIRB-10M16"]
["REIKU-B","VPIRB-10P07"]
["REIKU-B","VPIRB-10P09"]
["REIKU-B","VPIRB-10U05"]
["REIKU-B","VPIRB-10U07"]
["REIKU-B","VPIRB-12M16"]
["REIKU-B","VPIRB-12M20"]
["REIKU-B","VPIRB-12P11"]
["REIKU-B","VPIRB-12P13"]
["REIKU-B","VPIRB-12U05"]
["REIKU-B","VPIRB-12U06"]
["REIKU-B","VPIRB-12U07"]
["REIKU-B","VPIRB-12U09"]
["REIKU-B","VPIRB-12U10"]
["REIKU-B","VPIRB-17M20"]
["REIKU-B","VPIRB-17M25"]
["REIKU-B","VPIRB-17P13"]
["REIKU-B","VPIRB-17P16"]
["REIKU-B","VPIRB-17U07"]
["REIKU-B","VPIRB-17U09"]
["REIKU-B","VPIRB-17U10"]
["REIKU-B","VPIRB-17U11"]
["REIKU-B","VPIRB-17U14"]
["REIKU-B","VPIRB-17U17"]
["REIKU-B","VPIRB-23M25"]
["REIKU-B","VPIRB-23M32"]
["REIKU-B","VPIRB-23P21"]
["REIKU-B","VPIRB-23U14"]
["REIKU-B","VPIRB-23U17"]
["REIKU-B","VPIRB-23U18"]
["REIKU-B","VPIRB-29M32"]
["REIKU-B","VPIRB-29M40"]
["REIKU-B","VPIRB-29P29"]
["REIKU-B","VPIRB-29U24"]
["REIKU-B","VPIRB-36M40"]
["REIKU-B","VPIRB-36M50"]
["REIKU-B","VPIRB-36P36"]
["REIKU-B","VPIRB-48M50"]
["REIKU-B","VPIRB-48M63"]
["REIKU-B","VPIRB-48P48"]
["REIKU-G","VPIRG-10M121"]
["REIKU-G","VPIRG-10M16"]
["REIKU-G","VPIRG-10P07"]
["REIKU-G","VPIRG-10P09"]
["REIKU-G","VPIRG-10U05"]
["REIKU-G","VPIRG-10U07"]
["REIKU-G","VPIRG-12M16"]
["REIKU-G","VPIRG-12M20"]
["REIKU-G","VPIRG-12P11"]
["REIKU-G","VPIRG-12P13"]
["REIKU-G","VPIRG-12U05"]
["REIKU-G","VPIRG-12U06"]
["REIKU-G","VPIRG-12U07"]
["REIKU-G","VPIRG-12U09"]
["REIKU-G","VPIRG-12U10"]
["REIKU-G","VPIRG-17M20"]
["REIKU-G","VPIRG-17M25"]
["REIKU-G","VPIRG-17P13"]
["REIKU-G","VPIRG-17P16"]
["REIKU-G","VPIRG-17U07"]
["REIKU-G","VPIRG-17U09"]
["REIKU-G","VPIRG-17U10"]
["REIKU-G","VPIRG-17U11"]
["REIKU-G","VPIRG-17U14"]
["REIKU-G","VPIRG-17U17"]
["REIKU-G","VPIRG-23M25"]
["REIKU-G","VPIRG-23M32"]
["REIKU-G","VPIRG-23P21"]
["REIKU-G","VPIRG-23U14"]
["REIKU-G","VPIRG-23U17"]
["REIKU-G","VPIRG-23U18"]
["REIKU-G","VPIRG-29M32"]
["REIKU-G","VPIRG-29M40"]
["REIKU-G","VPIRG-29P29"]
["REIKU-G","VPIRG-29U24"]
["REIKU-G","VPIRG-36M40"]
["REIKU-G","VPIRG-36M50"]
["REIKU-G","VPIRG-36P36"]
["REIKU-G","VPIRG-48M50"]
["REIKU-G","VPIRG-48M63"]
["REIKU-G","VPIRG-48P48"]
["REIKU-B","VPIVB-36M40"]
["TECHNIK","VPK 100"]
["TECHNIK","VPK 120"]
["TECHNIK","VPK 150"]
["TECHNIK","VPK 180"]
["TECHNIK","VPK 226"]
["TECHNIK","VPK 280"]
["TECHNIK","VPKC 100"]
["TECHNIK","VPKC 120"]
["TECHNIK","VPKC 150"]
["TECHNIK","VPKC 180"]
["TECHNIK","VPKC 226"]
["TECHNIK","VPKC 280"]
["TECHNIK","VPM 2,5x100 sv.modrá"]
["TECHNIK","VPM 3,4x200 sv.modrá"]
["TECHNIK","VPM 4,8x190 sv.modrá"]
["TECHNIK","VPM 4,8x290 sv.modrá"]
["TECHNIK","VPM 4,8x370 sv.modrá"]
["TECHNIK","VPM 7,6x370 sv.modrá"]
["TECHNIK","VPM+ 2,5x100"]
["TECHNIK","VPM+ 3,6x200"]
["TECHNIK","VPM+ 4,6x200"]
["TECHNIK","VPM+ 4,8x190"]
["TECHNIK","VPM+ 4,8x300"]
["TECHNIK","VPM+ 4,8x370"]
["TECHNIK","VPN  2,5x100"]
["TECHNIK","VPN  2,5x160"]
["TECHNIK","VPN  3,6x150"]
["TECHNIK","VPN  3,6x200"]
["TECHNIK","VPN  3,6x290"]
["TECHNIK","VPN  4,8x200"]
["TECHNIK","VPN  4,8x300"]
["TECHNIK","VPN  4,8x370"]
["TECHNIK","VPP  1,7x70"]
["TECHNIK","VPP  1,9x100"]
["TECHNIK","VPP  2,4x60"]
["TECHNIK","VPP  2,4x80"]
["TECHNIK","VPP  2,5x100"]
["TECHNIK","VPP  2,5x100/1000"]
["TECHNIK","VPP  2,5x120"]
["TECHNIK","VPP  2,5x140"]
["TECHNIK","VPP  2,5x160"]
["TECHNIK","VPP  2,5x200"]
["TECHNIK","VPP  3,6x140"]
["TECHNIK","VPP  3,6x150"]
["TECHNIK","VPP  3,6x180"]
["TECHNIK","VPP  3,6x200"]
["TECHNIK","VPP  3,6x250"]
["TECHNIK","VPP  3,6x300"]
["TECHNIK","VPP  3,6x370"]
["TECHNIK","VPP  4,8x120"]
["TECHNIK","VPP  4,8x160"]
["TECHNIK","VPP  4,8x188"]
["TECHNIK","VPP  4,8x200"]
["TECHNIK","VPP  4,8x250"]
["TECHNIK","VPP  4,8x280"]
["TECHNIK","VPP  4,8x300"]
["TECHNIK","VPP  4,8x370"]
["TECHNIK","VPP  4,8x430"]
["TECHNIK","VPP  4,8x530"]
["TECHNIK","VPP  4,8x680"]
["TECHNIK","VPP  4,8x830"]
["TECHNIK","VPP  7,6x150"]
["TECHNIK","VPP  7,6x200"]
["TECHNIK","VPP  7,6x240"]
["TECHNIK","VPP  7,6x300"]
["TECHNIK","VPP  7,6x370"]
["TECHNIK","VPP  7,8x450"]
["TECHNIK","VPP  7,8x550"]
["TECHNIK","VPP  7,8x750"]
["TECHNIK","VPP  9,0x 430"]
["TECHNIK","VPP  9,0x 530"]
["TECHNIK","VPP  9,0x 780"]
["TECHNIK","VPP  9,0x1020"]
["TECHNIK","VPP  9,0x1220"]
["TECHNIK","VPP  9,0x1530"]
["TECHNIK","VPP 13x 230"]
["TECHNIK","VPP 13x 380"]
["TECHNIK","VPP 13x 480"]
["TECHNIK","VPP 13x 580"]
["TECHNIK","VPP 13x 730"]
["TECHNIK","VPP 13x 830"]
["TECHNIK","VPP 13x1000"]
["TECHNIK","VPPFE 2,4x 90"]
["TECHNIK","VPPFE 2,4x200"]
["TECHNIK","VPPFE 2,4x360"]
["TECHNIK","VPPFE 3,6x140"]
["TECHNIK","VPPFE 3,6x200"]
["TECHNIK","VPPFE 3,6x280"]
["TECHNIK","VPPFE 3,6x370"]
["TECHNIK","VPPFE 4,8x180"]
["TECHNIK","VPPFE 4,8x290"]
["TECHNIK","VPPFE 4,8x360"]
["TECHNIK","VPPFE 7,6x340"]
["TECHNIK","VPPFE 7,6x760"]
["TECHNIK","VPR+ 2,5x100"]
["TECHNIK","VPR+ 2,5x140"]
["TECHNIK","VPR+ 2,5x160"]
["TECHNIK","VPR+ 3,6x140"]
["TECHNIK","VPR+ 3,6x200"]
["TECHNIK","VPR+ 3,6x300"]
["TECHNIK","VPR+ 3,6x360"]
["TECHNIK","VPR+ 4,8x200"]
["TECHNIK","VPR+ 4,8x250"]
["TECHNIK","VPR+ 4,8x290"]
["TECHNIK","VPR+ 4,8x360"]
["TECHNIK","VPR+ 4,8x430"]
["TECHNIK","VPR+ 4,8x530"]
["TECHNIK","VPR+ 7,6x250"]
["TECHNIK","VPR+ 7,6x360"]
["TECHNIK","VPRO 3,6x100"]
["TECHNIK","VPRO 4,8x150"]
["TECHNIK","VPRO 4,8x200"]
["TECHNIK","VPRO 4,8x250"]
["TECHNIK","VPRO 4,8x300"]
["TECHNIK","VPRO 4,8x370"]
["TECHNIK","VPRO 7,6x120"]
["TECHNIK","VPRO 7,6x150"]
["TECHNIK","VPRO 7,6x200"]
["TECHNIK","VPRO 7,6x300"]
["TECHNIK","VPRO12,4x400"]
["TECHNIK","VPRO12,4x500"]
["TECHNIK","VPS  2,5x100"]
["TECHNIK","VPS  2,5x110"]
["TECHNIK","VPS  2,5x130"]
["TECHNIK","VPS  2,5x200"]
["TECHNIK","VPS  2,5x210"]
["TECHNIK","VPS  4,8x220"]
["TECHNIK","VPS  4,8x270"]
["TECHNIK","VPS  4,8x300"]
["TECHNIK","VPS  4,8x370"]
["TECHNIK","VPS3  4,8x220"]
["TECHNIK","VPSO 2,5x110"]
["TECHNIK","VPSO 3,6x150"]
["TECHNIK","VPSO 4,8x200"]
["TECHNIK","VPSO 4,8x300"]
["TECHNIK","VPSO 4,8x370"]
["TECHNIK","VPSO 7,6x200"]
["TECHNIK","VPSO 7,6x300"]
["TECHNIK","VPSO 7,6x370"]
["TECHNIK","VPSO 7,9x400"]
["REIKU-B","VPSRB-10M12"]
["REIKU-B","VPSRB-10M16"]
["REIKU-B","VPSRB-10M20"]
["REIKU-B","VPSRB-12M20"]
["REIKU-G","VPSRG-10M12"]
["REIKU-G","VPSRG-10M16"]
["REIKU-G","VPSRG-10M20"]
["REIKU-G","VPSRG-12M20"]
["TECHNIK","VPST 4,5x 100"]
["TECHNIK","VPST 4,5x 127"]
["TECHNIK","VPST 4,5x 152"]
["TECHNIK","VPST 4,5x 200"]
["TECHNIK","VPST 4,5x 200/316"]
["TECHNIK","VPST 4,5x 265"]
["TECHNIK","VPST 4,5x 300"]
["TECHNIK","VPST 4,5x 360"]
["TECHNIK","VPST 4,5x 520"]
["TECHNIK","VPST 4,5x 680"]
["TECHNIK","VPST 4,5x 840"]
["TECHNIK","VPST 4,5x1060"]
["TECHNIK","VPST 4,5x1190"]
["TECHNIK","VPST 6,3x 150 NL"]
["TECHNIK","VPST 6,3x 230 NL"]
["TECHNIK","VPST 6,3x 300 NL"]
["TECHNIK","VPST 8x 152"]
["TECHNIK","VPST 8x 152 EX"]
["TECHNIK","VPST 8x 200"]
["TECHNIK","VPST 8x 200 EX"]
["TECHNIK","VPST 8x 200 NL"]
["TECHNIK","VPST 8x 265"]
["TECHNIK","VPST 8x 265 EX"]
["TECHNIK","VPST 8x 300"]
["TECHNIK","VPST 8x 300 EX"]
["TECHNIK","VPST 8x 300 PR"]
["TECHNIK","VPST 8x 360"]
["TECHNIK","VPST 8x 360 EX"]
["TECHNIK","VPST 8x 360 NL"]
["TECHNIK","VPST 8x 520"]
["TECHNIK","VPST 8x 520 EX"]
["TECHNIK","VPST 8x 520 NL"]
["TECHNIK","VPST 8x 680"]
["TECHNIK","VPST 8x 680 EX"]
["TECHNIK","VPST 8x 840"]
["TECHNIK","VPST 8x 840 EX"]
["TECHNIK","VPST 8x1060"]
["TECHNIK","VPST 8x1060 EX"]
["REIKU-B","VPSVB-10M12"]
["REIKU-B","VPSVB-10M16"]
["REIKU-B","VPSVB-10M20"]
["REIKU-B","VPSVB-12M20"]
["REIKU-G","VPSVG-10M12"]
["REIKU-G","VPSVG-10M16"]
["REIKU-G","VPSVG-10M20"]
["REIKU-G","VPSVG-12M20"]
["TECHNIK","VPZIP 13x150"]
["TECHNIK","VPZIP 13x200 bílá"]
["TECHNIK","VPZIP 13x200 černá"]
["TECHNIK","VPZIP 13x200 modrá"]
["TECHNIK","VPZIP 13x200 rudá"]
["TECHNIK","VPZIP 13x250"]
["TECHNIK","VPZIP 20x300"]
["TECHNIK","VPZIP 30x400"]
["TECHNIK","VPZIP 30x600"]
["TECHNIK","VPZIP-100"]
["TECHNIK","VPZIP-12"]
["TECHNIK","VPZIP-20"]
["TECHNIK","VPZIP-20 S"]
["TECHNIK","VPZIP-25"]
["TECHNIK","VPZIP-50"]
["TECHNIK","VPŽDO 2,5x110"]
["TECHNIK","VRE 0104"]
["TECHNIK","VRE 0204"]
["TECHNIK","VRE 0304"]
["TECHNIK","VRE 0404"]
["TECHNIK","VRE 0504"]
["TECHNIK","VRE 0524"]
["TECHNIK","VRE 0534"]
["TECHNIK","VRE 0554"]
["TECHNIK","VRE 0604"]
["TECHNIK","VRE 0704"]
["TECHNIK","VRE 0714"]
["TECHNIK","VRE 0754"]
["TECHNIK","VRE 0804"]
["TECHNIK","VRE 0904"]
["TECHNIK","VRE 1004"]
["TECHNIK","VRE 1014"]
["TECHNIK","VRE 1104"]
["TECHNIK","VRE 1204"]
["TECHNIK","VRE kufr"]
["TECHNIK SPECIAL - AKCIA","VRTÁK 10,0"]
["TECHNIK SPECIAL - AKCIA","VRTÁK 11,5"]
["TECHNIK","VS  4-12"]
["TECHNIK","VS  6-20"]
["TECHNIK","VS  6-30"]
["TECHNIK","VS 30-40"]
["TECHNIK","VS 40-50"]
["TECHNIK","VS 50-60"]
["TECHNIK","VS AM"]
["TECHNIK","VS AM-1"]
["TECHNIK","VS AM-TIN"]
["TECHNIK","VS MF"]
["TECHNIK","VS PG"]
["TECHNIK","VS PVD"]
["TECHNIK","VS PVD-TIN"]
["TECHNIK","VS PVK"]
["TECHNIK","VS SET 4-30"]
["TECHNIK","VS-hlavička"]
["TECHNIK","VS-komplet"]
["TECHNIK","VS-nůž"]
["TECHNIK","VS-páska bílá"]
["TECHNIK","VS-páska černá"]
["TECHNIK","VS-spona bílá"]
["TECHNIK","VS-spona černá"]
["TECHNIK","VULCANE EXPRES"]
["TECHNIK","VULK 19x3,5 NN"]
["TECHNIK","VULK 19x7,5"]
["TECHNIK","VULK 19x7,5 NN"]
["TECHNIK","VULK 25x10 NN"]
["TECHNIK","VULK 25x5 NN"]
["TECHNIK","VULK 25x7,5"]
["TECHNIK","VULK 25x7,5 NN"]
["TECHNIK","VULK 50x7,5"]
["TECHNIK","VULK 50x7,5 NN"]
["TECHNIK","W1   8-12"]
["TECHNIK","W1  10-16"]
["TECHNIK","W1  12-20"]
["TECHNIK","W1  16-25"]
["TECHNIK","W1  20-32"]
["TECHNIK","W1  25-40"]
["TECHNIK","W1  32-50"]
["TECHNIK","W1  40-60"]
["TECHNIK","W1  50-70"]
["TECHNIK","W1  60-80"]
["TECHNIK","W2  50-70"]
["TECHNIK","W44T Turbo"]
["TECHNIK SPECIAL - AKCIA","WA10A"]
["TECHNIK SPECIAL - AKCIA","WA22P"]
["TECHNIK SPECIAL - AKCIA","WA23"]
["TECHNIK SPECIAL - AKCIA","WA23-10"]
["TECHNIK SPECIAL - AKCIA","WA23-2"]
["TECHNIK SPECIAL - AKCIA","WA23-3"]
["TECHNIK SPECIAL - AKCIA","WA23-9"]
["TECHNIK SPECIAL - AKCIA","WA27F"]
["TECHNIK","WC-100"]
["TECHNIK","WE 1,5"]
["TECHNIK","WE 13"]
["TECHNIK","WE 2"]
["TECHNIK","WE 25"]
["TECHNIK","WE 28-35"]
["TECHNIK","WE 3"]
["TECHNIK","WE 35-50"]
["TECHNIK","WE 4-16"]
["TECHNIK","WE 4-28G"]
["TECHNIK","WE 4-28H"]
["TECHNIK","WE 5"]
["TECHNIK","WE 5/1000"]
["TECHNIK","WE 7F"]
["TECHNIK","WE 7R"]
["TECHNIK","WE 7S"]
["TECHNIK","WE 8-27"]
["TECHNIK","WE100"]
["TECHNIK","WE150"]
["TECHNIK","WE200"]
["TECHNIK","WE300"]
["TECHNIK","WE400"]
["TECHNIK","WE500"]
["TECHNIK","WH 00883"]
["TECHNIK","WH 00884"]
["TECHNIK","WH 00885"]
["TECHNIK","WH 00888"]
["TECHNIK","WH 00889"]
["TECHNIK","WH 03763"]
["TECHNIK","WR 003484"]
["TECHNIK","WR 003544"]
["TECHNIK","WR 005315"]
["TECHNIK","WR 005325"]
["TECHNIK","WR 006184"]
["TECHNIK","WR 008775"]
["TECHNIK","WR 008780"]
["TECHNIK","WR 017005"]
["TECHNIK","WR 017010"]
["TECHNIK","WR 017015"]
["TECHNIK","WR 018260"]
["TECHNIK","WR 018262"]
["TECHNIK","WR 018264"]
["TECHNIK","WR 018266"]
["TECHNIK","WR 018268"]
["TECHNIK","WR 018282"]
["TECHNIK","WR 018287"]
["TECHNIK","WR 022086"]
["TECHNIK","WR 022800"]
["TECHNIK","WR 022805"]
["TECHNIK","WR 023105"]
["TECHNIK","WR 031200"]
["TECHNIK","WR 031209"]
["TECHNIK","WR 031210"]
["TECHNIK","WR 031211"]
["TECHNIK","WR 031212"]
["TECHNIK","WR 031219"]
["TECHNIK","WR 031220"]
["TECHNIK","WR 031221"]
["TECHNIK","WR 031225"]
["TECHNIK","WR 031226"]
["TECHNIK","WR 031401"]
["TECHNIK","WR 031402"]
["TECHNIK","WR 031408"]
["TECHNIK","WR 031412"]
["TECHNIK","WR 031415"]
["TECHNIK","WR 031427"]
["TECHNIK","WR 031440"]
["TECHNIK","WR 031441"]
["TECHNIK","WR 031442"]
["TECHNIK","WR 031444"]
["TECHNIK","WR 031445"]
["TECHNIK","WR 031451"]
["TECHNIK","WR 031461"]
["TECHNIK","WR 031501"]
["TECHNIK","WR 031502"]
["TECHNIK","WR 031503"]
["TECHNIK","WR 031504"]
["TECHNIK","WR 031505"]
["TECHNIK","WR 031506"]
["TECHNIK","WR 031575"]
["TECHNIK","WR 031576"]
["TECHNIK","WR 051019"]
["TECHNIK","WR 052490"]
["TECHNIK","WR 052502"]
["TECHNIK","WR 053457"]
["TECHNIK","WR 053459"]
["TECHNIK","WR 056168"]
["TECHNIK","WR 056200"]
["TECHNIK","WR 056295"]
["TECHNIK","WR 056303"]
["TECHNIK","WR 056305"]
["TECHNIK","WR 056310"]
["TECHNIK","WR 056315"]
["TECHNIK","WR 056320"]
["TECHNIK","WR 056325"]
["TECHNIK","WR 056330"]
["TECHNIK","WR 056332"]
["TECHNIK","WR 056335"]
["TECHNIK","WR 056340"]
["TECHNIK","WR 056500"]
["TECHNIK","WR 056505"]
["TECHNIK","WR 056507"]
["TECHNIK","WR 056510"]
["TECHNIK","WR 056525"]
["TECHNIK","WR 056605"]
["TECHNIK","WR 056610"]
["TECHNIK","WR 056625"]
["TECHNIK","WR 056910"]
["TECHNIK","WR 056915"]
["TECHNIK","WR 056925"]
["TECHNIK","WR 057126"]
["TECHNIK","WR 057705"]
["TECHNIK","WR 060110"]
["TECHNIK","WR 060402"]
["TECHNIK","WR 060403"]
["TECHNIK","WR 066485"]
["TECHNIK","WR 066486"]
["TECHNIK","WR 066487"]
["TECHNIK","WR 066488"]
["TECHNIK","WR 066489"]
["TECHNIK","WR 066490"]
["TECHNIK","WR 066491"]
["TECHNIK","WR 066492"]
["TECHNIK","WR 066493"]
["TECHNIK","WR 066494"]
["TECHNIK","WR 066495"]
["TECHNIK","WR 066496"]
["TECHNIK","WR 071071"]
["TECHNIK","WR 071072"]
["TECHNIK","WR 071074"]
["TECHNIK","WR 072050"]
["TECHNIK","WR 072055"]
["TECHNIK","WR 072057"]
["TECHNIK","WR 072059"]
["TECHNIK","WR 072061"]
["TECHNIK","WR 072063"]
["TECHNIK","WR 072065"]
["TECHNIK","WR 072070"]
["TECHNIK","WR 072072"]
["TECHNIK","WR 072074"]
["TECHNIK","WR 072082"]
["TECHNIK","WR 073593"]
["TECHNIK","WR 110069"]
["TECHNIK","WR 118150"]
["TECHNIK","WR 118152"]
["TECHNIK","WR 134480"]
["TECHNIK","WR 138070"]
["TECHNIK","WT 1"]
["TECHNIK","WT 110"]
["TECHNIK","WT 110 P"]
["TECHNIK","WT 60"]
["TECHNIK","WT 85"]
["TECHNIK","XR- 6WE1"]
["TECHNIK","XR- 6WE1.C"]
["TECHNIK","XR- 6YW1.C"]
["TECHNIK","XR- 9BU1"]
["TECHNIK","XR- 9GN1"]
["TECHNIK","XR- 9RD1"]
["TECHNIK","XR- 9SR1"]
["TECHNIK","XR- 9WE1"]
["TECHNIK","XR- 9WE1.C"]
["TECHNIK","XR- 9X1"]
["TECHNIK","XR- 9X1.C"]
["TECHNIK","XR- 9YW1"]
["TECHNIK","XR- 9YW1.C"]
["TECHNIK","XR-12WE1"]
["TECHNIK","XR-12WE1.C"]
["TECHNIK","XR-12X1.C"]
["TECHNIK","XR-12YW1"]
["TECHNIK","XR-12YW1.C"]
["TECHNIK","XR-18BU1"]
["TECHNIK","XR-18GN1"]
["TECHNIK","XR-18RD1"]
["TECHNIK","XR-18SR1"]
["TECHNIK","XR-18WE1"]
["TECHNIK","XR-18WE1.C"]
["TECHNIK","XR-18X1"]
["TECHNIK","XR-18YW1"]
["TECHNIK","XR-18YW1.C"]
["TECHNIK","XR-24WE1"]
["TECHNIK","XR-24WE1.C"]
["TECHNIK","XR-24YW1"]
["TECHNIK","XR-24YW1.C"]
["ABTECH","ZAG 1"]
["ABTECH","ZAG 10"]
["ABTECH","ZAG 10.9"]
["ABTECH","ZAG 11"]
["ABTECH","ZAG 12"]
["ABTECH","ZAG 13"]
["ABTECH","ZAG 14"]
["ABTECH","ZAG 15"]
["ABTECH","ZAG 16"]
["ABTECH","ZAG 17"]
["ABTECH","ZAG 18"]
["ABTECH","ZAG 18.3"]
["ABTECH","ZAG 19"]
["ABTECH","ZAG 2"]
["ABTECH","ZAG 20"]
["ABTECH","ZAG 21"]
["ABTECH","ZAG 22"]
["ABTECH","ZAG 3"]
["ABTECH","ZAG 4"]
["ABTECH","ZAG 5"]
["ABTECH","ZAG 6"]
["ABTECH","ZAG 7"]
["ABTECH","ZAG 8"]
["ABTECH","ZAG 9"]
["ABTECH","ZAG 9.9"]
["ABTECH","ZAG-EX 10"]
["ABTECH","ZAG-EX 10.9"]
["ABTECH","ZAG-EX 11"]
["ABTECH","ZAG-EX 12"]
["ABTECH","ZAG-EX 13"]
["ABTECH","ZAG-EX 15"]
["ABTECH","ZAG-EX 16"]
["ABTECH","ZAG-EX 2"]
["ABTECH","ZAG-EX 3"]
["ABTECH","ZAG-EX 4"]
["ABTECH","ZAG-EX 5"]
["ABTECH","ZAG-EX 6"]
["ABTECH","ZAG-EX 7"]
["ABTECH","ZAG-EX 9"]
["ABTECH","ZAG-EX 9.9"]
["TECHNIK SPECIAL - AKCIA","ZDBX  1"]
["TECHNIK SPECIAL - AKCIA","ZDBX  3"]
["TECHNIK SPECIAL - AKCIA","ZDBX  4"]
["TECHNIK SPECIAL - AKCIA","ZDBX 11"]
["TECHNIK SPECIAL - AKCIA","ZDBX 15"]
["TECHNIK SPECIAL - AKCIA","ZDBX 16"]
["TECHNIK SPECIAL - AKCIA","ZDBX 20"]
["TECHNIK","ZH-PUR 100"]
["TECHNIK","ZH-PUR 230"]
["TECHNIK","ZH-PUR 426"]
["TECHNIK","ZID4-M"]
["TECHNIK","ZID4-M žz"]
["TECHNIK","ZID4-M0"]
["TECHNIK","ZID4-M0 žz"]
["TECHNIK","ZID4-M1"]
["TECHNIK","ZID4-M1 žz"]
["TECHNIK","ZID4-M2"]
["TECHNIK","ZID4-M2 žz"]
["TECHNIK","ZID4-M3"]
["TECHNIK","ZID4-M3 žz"]
["TECHNIK","ZID4-M4"]
["TECHNIK","ZID4-M5"]
["TECHNIK","ZID5-M"]
["TECHNIK","ZID5-M žz"]
["TECHNIK","ZID5-M0"]
["TECHNIK","ZID5-M0 žz"]
["TECHNIK","ZID5-M1"]
["TECHNIK","ZID5-M1 žz"]
["TECHNIK","ZID5-M2"]
["TECHNIK","ZID5-M2 žz"]
["TECHNIK","ZID5-M3 žz"]
["TECHNIK","Zinkohliníkový sprej"]
["TECHNIK","Zinkový sprej"]
["REIKU-B","ZKDRB-42"]
["REIKU-B","ZKDRB-52"]
["REIKU-B","ZKDRB-70"]
["REIKU-B","ZKDRB-95"]
["ABTECH","ZP 1"]
["ABTECH","ZP 10"]
["ABTECH","ZP 11"]
["ABTECH","ZP 11.9 Shr"]
["ABTECH","ZP 12"]
["ABTECH","ZP 13"]
["ABTECH","ZP 14"]
["ABTECH","ZP 15"]
["ABTECH","ZP 16"]
["ABTECH","ZP 17"]
["ABTECH","ZP 18"]
["ABTECH","ZP 19"]
["ABTECH","ZP 2"]
["ABTECH","ZP 21 Shr"]
["ABTECH","ZP 22 Shr"]
["ABTECH","ZP 24 Shr"]
["ABTECH","ZP 25 Shr"]
["ABTECH","ZP 26 Shr"]
["ABTECH","ZP 3"]
["ABTECH","ZP 4"]
["ABTECH","ZP 5"]
["ABTECH","ZP 6"]
["ABTECH","ZP 7"]
["ABTECH","ZP 8"]
["ABTECH","ZP 9"]
["ABTECH","ZPS 1"]
["ABTECH","ZPS 10"]
["ABTECH","ZPS 11"]
["ABTECH","ZPS 11.9 Shr"]
["ABTECH","ZPS 12"]
["ABTECH","ZPS 13"]
["ABTECH","ZPS 14"]
["ABTECH","ZPS 15"]
["ABTECH","ZPS 16"]
["ABTECH","ZPS 17"]
["ABTECH","ZPS 18"]
["ABTECH","ZPS 19"]
["ABTECH","ZPS 2"]
["ABTECH","ZPS 21 Shr"]
["ABTECH","ZPS 22 Shr"]
["ABTECH","ZPS 24 Shr"]
["ABTECH","ZPS 25 Shr"]
["ABTECH","ZPS 26 Shr"]
["ABTECH","ZPS 3"]
["ABTECH","ZPS 4"]
["ABTECH","ZPS 5"]
["ABTECH","ZPS 6"]
["ABTECH","ZPS 7"]
["ABTECH","ZPS 8"]
["ABTECH","ZPS 9"]
["TECHNIK","ZS 1"]
["TECHNIK","ZS 2,5"]
["TECHNIK","ZS 6"]
["TECHNIK","ZSD 1"]
["TECHNIK","ZSD 2,5"]
["TECHNIK","ZSD 4"]
["TECHNIK","ZSP 2"]
["TECHNIK","Z-TESTER"]
["ABTECH"]